{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Factor Summary","data included","data excluded"],"read":"whole","date_system":"1900"}

{"sheet":"Factor Summary","index":0,"n_rows":13,"n_cols":2,"rows_kept":13}
["Key Parameters","Results"]
["SCC",30500623]
["Does the SCC contain more than 15 sources?","Yes"]
["Pollutant","NITROGEN OXIDES (NOX)"]
["Units","LB"]
["Activity","TONS CLINKER PRODUCED"]
["Factor Quality Rating","Moderately "]
["Number of individual test data values used to calculate the emissions factor",9]
["Number of individual test data values excluded from the calculation",15]
["Composite Test Rating",68.31]
["Control Device Configuration","FABRIC FILTER"]
["New Candidate Factor Value ",{"v":4.1,"d":"4.10E+00"}]
["AP42 Section ",11.6]

{"sheet":"data included","index":1,"n_rows":10,"n_cols":11,"rows_kept":10}
["Individual Test Data Value","Individual Test Method","Individual Test Data Units","Individual Test Data Activity","Individual Test Rating","Detection Limit Flag ","Year of Test","Facility Name","Test City","Test State","ERT Project Data Set"]
[{"v":4.13,"d":"4.13E+00"},"Method 7E","LB","TONS CLINKER PRODUCED",78.5,"ADL",2016,"Monarch Cement Company","Humboldt","KS","PDS"]
[{"v":4.09,"d":"4.09E+00"},"Method 7E","LB","TONS CLINKER PRODUCED",78.5,"ADL",2015,"Monarch Cement Company","Humboldt","KS","PDS"]
[{"v":3.64,"d":"3.64E+00"},"Method 7E","LB","TONS CLINKER PRODUCED",78.5,"ADL",2017,"Monarch Cement Company - Humboldt Kansas","Humboldt","KS","PDS"]
[{"v":3.22,"d":"3.22E+00"},"Method 7E","LB","TONS CLINKER PRODUCED",78.5,"ADL",2020,"Monarch Cement Company - Humboldt Kansas","Humboldt","KS","PDS"]
[{"v":3.21,"d":"3.21E+00"},"Method 7E","LB","TONS CLINKER PRODUCED",77,"ADL",2018,"Monarch Cement Company - Humboldt Kansas","Humboldt","KS","PDS"]
[{"v":6.5,"d":"6.50E+00"},"Continuous Emissions","LB","TONS CLINKER PRODUCED",60,"ADL",null,"Southwestern Portland Cement","Victorville","CA","PDS"]
[{"v":4.25,"d":"4.25E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",60,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
[{"v":4.1,"d":"4.10E+00"},"Continuous Emissions","LB","TONS CLINKER PRODUCED",60,"ADL",null,"Southwestern Portland Cement","Victorville","CA","PDS"]
[{"v":3.74,"d":"3.74E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",60,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]

{"sheet":"data excluded","index":2,"n_rows":16,"n_cols":12,"rows_kept":16}
["Reason for Exclusion","Individual Test Data Value","Individual Test Method","Individual Test Data Units","Individual Test Data Activity","Individual Test Rating","Detection Limit Flag ","Year of Test","Facility Name","Test City","Test State","ERT Project Data Set"]
["Data value is an outlier.",{"v":0.614,"d":"6.14E-01"},"Method 7E","LB","TONS CLINKER PRODUCED",78.5,"ADL",2017,"LaFarge Building Materials - Ravena Facility","Ravena","NY","PDS"]
["Data value is an outlier.",{"v":0.614,"d":"6.14E-01"},"Method 7E","LB","TONS CLINKER PRODUCED",78.5,"ADL",2017,"LaFarge Building Materials - Ravena Facility","Ravena","NY","PDS"]
["Data value does not improve the factor quality rating.",{"v":9.5,"d":"9.50E+00"},"EPA Method 7","LB","TONS CLINKER PRODUCED",45,"ADL",null,"Southwestern Cement","Leamington","UT","PDS"]
["Data value does not improve the factor quality rating.",{"v":9.5,"d":"9.50E+00"},"EPA Method 7","LB","TONS CLINKER PRODUCED",45,"ADL",null,"Southwestern Cement","Leamington","UT","PDS"]
["Data value does not improve the factor quality rating.",{"v":5.5,"d":"5.50E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":5.3,"d":"5.30E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":4.5,"d":"4.50E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":3.9,"d":"3.90E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":3.4,"d":"3.40E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":3.06,"d":"3.06E+00"},"Continuous Emissions","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":2.8,"d":"2.80E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value is an outlier.",{"v":1.7,"d":"1.70E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",45,"ADL",null,"California Portland Cement","Mojave","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":6.6,"d":"6.60E+00"},"CARB Method 1-100","LB","TONS CLINKER PRODUCED",30,"ADL",null,"Southwestern Portland Cement","Victorville","CA","PDS"]
["Data value does not improve the factor quality rating.",{"v":4.4,"d":"4.40E+00"},"Not available","LB","TONS CLINKER PRODUCED",30,"ADL",null,"Ash Grove Cement West, Inc","Portland","OR","PDS"]
["EPA Manually Excluded - Duplicate Report",{"v":4.09,"d":"4.09E+00"},"Method 7E","LB","TONS CLINKER PRODUCED",78.5,"ADL",2015,"Monarch Cement Company","Humboldt","KS","PDS"]