{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Family Info","ESRI_MAPINFO_SHEET"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Family Info","index":0,"n_rows":216817,"n_cols":36,"rows_kept":2250,"cut":true,"bounds":{"rows_first":1000,"rows_last":250,"rows_between":1000,"halvings":1}}
[]
["Model Year","Manufacturer Name","Vehicle Family","Vehicle Subcategory","Certificate Number","Vehicle Trade Name","Fuel Type","Useful LIfe","ABT Y/N","Evap System Y/N","CO2 Standard (g/ton-mile)","Lowest Projected CO2 FEL (g/ton-mile)","Highest Projected CO2 FEL (g/ton-mile)","Typical Application Description","EPA Assigned DF Y/N","Additive DF Value","Multiplicative DF Value","Adjustable Parameters Y/N","AECDs Y/N","Vehicle Speed Limiter Y/N","Auto Engine Shutdown (AES) Y/N","Engine Shutdown Conditions","Innovative Tech Y/N","Innovative Tech Name","Innovative Tech Description","Advanced Tech Y/N","Advanced Tech Type","AES Override Conditions","High Roof Sleeper CDA Measurement","High Roof Sleeper Vehicle Family Name","Wheel Weight Reduction Y/N","Nonwheel Weight Reduction Y/N","IT Weight Reduction Y/N","A/C System Y/N","Introduction to Commerce","Emission Control System"]
[2025,"The Lion Electric Co USA","SLEL2VOCVLC1","School bus","SLEL2VOCVLC1-001","LIONC","Electricity","10 years / 185,000 mi","N","N",291,0,0,"TYPE C SCHOOL BUS","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-05-15","Low rolling resistance tires (all)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FDB6000","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"The Lion Electric Co USA","SLEL2VOCVL5P","Compression-ignition Medium HDV - Multipurpose","SLEL2VOCVL5P-003","LION5","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"Class 5 & 6 straight body truck","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-05-27","Low rolling resistance tires (all)"]
[2025,"The Lion Electric Co USA","SLEL2VOCVL8P","Compression-ignition Heavy HDV - Multipurpose","SLEL2VOCVL8P-004","LION8 - STRAIGHT TRUCK","Electricity","10 years / 435,000 mi","N","N",242,0,0,"Class 8 straight body truck","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-05-27","Low rolling resistance tires (all)"]
[2025,"Daimler Coaches North America","SRCC2VOCV001","Coach bus","SRCC2VOCV001-001","Mercedes Benz Tourrider","Diesel","10 years / 435,000 mi","N","N",210,202,206,"Over the road luxury motorcoach commonly found in the premium tour and charter market segments.","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","N","N","Y","2024-09-01","Low rolling resistance tires (all)"]
[2025,"The Lion Electric Co USA","SLEL2VOCVL5A","Compression-ignition Light HDV - Multipurpose","SLEL2VOCVL5A-006","LION5","Electricity","15 years / 150,000 mi","Y","N",344,0,0,"Class 5 straight body truck","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-06-10","Low rolling resistance tires (all)"]
[2025,"Bollinger Motors LLC","SBOL2VOCVB40","Compression-ignition Light HDV - Multipurpose","SBOL2VOCVB40-001","Bollinger Motors B4","Electricity","15 years / 150,000 mi","Y","N",344,0,0,"BEV vehicles built as Incomplete Light-HDV Chassis Cabs which are then distributed to dealerships or upfitters to be completed to suit the end-user's needs.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-16","Low rolling resistance tires (all)"]
[2025,"The Lion Electric Co USA","SLEL2VOCVL6P","Compression-ignition Medium HDV - Multipurpose","SLEL2VOCVL6P-005","LION6","Electricity","10 years / 185,000 mi","N","N",246,0,0,"Class 6 straight body truck","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-05-24","Low rolling resistance tires (all)"]
[2025,"Rosenbauer International AG","SRIA2VOCVEMR","Emergency vehicle","SRIA2VOCVEMR-001","Emergency Vehicle","Electricity","10 years / 435,000 mi","N","N",{"$nulls":3},"Hybrid-Electric Fire Truck","N",null,1,"N","N",{"$nulls":14},"Y","2024-03-20","Low rolling resistance tires (all)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e16M","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Low rolling resistance tires (all)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e16M","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18Lx","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Low rolling resistance tires (all)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18Lx","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e16L","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Low rolling resistance tires (all)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e16L","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18Mx","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Low rolling resistance tires (all)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18Mx","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18L","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Low rolling resistance tires (all)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18L","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18M","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Low rolling resistance tires (all)"]
[2025,"Mitsubishi Fuso Truck and Bus Corporation","SMFB2VOCV03B","Compression-ignition Medium HDV - Multipurpose","SMFB2VOCV03B-001","RIZON e18M","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"¿ Logistics/Transport/Parcel ¿ Dry containers ¿ Food and Perishables ¿ Reefer containers ¿ Municipal Application ¿ Flat beds/Special equipment like garbage compactor","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-09-01","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2025,"The Lion Electric Co USA","SLEL2TRACL8T","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","SLEL2TRACL8T-007","LION8T - TRACTOR TRUCK","Electricity","10 years / 435,000 mi","N","N",80.4,0,0,"Class 8 tractor truck","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-07-31","Low rolling resistance tires (all)"]
[2025,"Hyundai Motor Company","SHYX2TRACA32","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","SHYX2TRACA32-001","XCIENT FUEL CELL","Hydrogen","10 years / 435,000 mi","Y","N",80.4,0,0,null,"N",0,null,"N","N","N",null,null,"N",null,null,"Y","Fuel Cell Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-30","Aerodynamic roof fairing"]
[2025,"Hyundai Motor Company","SHYX2TRACA32","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","SHYX2TRACA32-001","XCIENT FUEL CELL","Hydrogen","10 years / 435,000 mi","Y","N",80.4,0,0,null,"N",0,null,"N","N","N",null,null,"N",null,null,"Y","Fuel Cell Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-30","Low rolling resistance tires (drive)"]
[2025,"Hyundai Motor Company","SHYX2TRACA32","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","SHYX2TRACA32-001","XCIENT FUEL CELL","Hydrogen","10 years / 435,000 mi","Y","N",80.4,0,0,null,"N",0,null,"N","N","N",null,null,"N",null,null,"Y","Fuel Cell Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-30","Low rolling resistance tires (steer)"]
[2025,"Hyundai Motor Company","SHYX2TRACA32","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","SHYX2TRACA32-001","XCIENT FUEL CELL","Hydrogen","10 years / 435,000 mi","Y","N",80.4,0,0,null,"N",0,null,"N","N","N",null,null,"N",null,null,"Y","Fuel Cell Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-30","Aerodynamic side skirt and/or fuel tank fairing"]
[2025,"Hyundai Motor Company","SHYX2TRACA32","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","SHYX2TRACA32-001","XCIENT FUEL CELL","Hydrogen","10 years / 435,000 mi","Y","N",80.4,0,0,null,"N",0,null,"N","N","N",null,null,"N",null,null,"Y","Fuel Cell Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-30","Gap reducing fairing"]
[2025,"ENVIROTECH DRIVE SYSTEMS INC","SETD2VOCVEBB","Compression-ignition Heavy HDV - Urban","SETD2VOCVEBB-002","Bumble Bee","Electricity","10 years / 435,000 mi","Y","N",283,0,0,"Phase 2 GHG Heavy HDV Family. The EVT Bumble Bee is a complete battery-electric HHD Class 8 school bus. This vehicle is all-electric with zero tailpipe emissions.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVLHD","Compression-ignition Light HDV - Multipurpose","SHBG2VOCVLHD-001","HBG-04","Electricity","15 years / 150,000 mi","Y","N",344,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVLHD","Compression-ignition Light HDV - Multipurpose","SHBG2VOCVLHD-001","HBG-04","Electricity","15 years / 150,000 mi","Y","N",344,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","N","N","Y","2024-11-01","Vehicle weight reduction"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVLHD","Compression-ignition Light HDV - Multipurpose","SHBG2VOCVLHD-001","HBG-05","Electricity","15 years / 150,000 mi","Y","N",344,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVLHD","Compression-ignition Light HDV - Multipurpose","SHBG2VOCVLHD-001","HBG-05","Electricity","15 years / 150,000 mi","Y","N",344,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","N","N","Y","2024-11-01","Vehicle weight reduction"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVMHD","Compression-ignition Medium HDV - Multipurpose","SHBG2VOCVMHD-002","HBG-07","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVMHD","Compression-ignition Medium HDV - Multipurpose","SHBG2VOCVMHD-002","HBG-07","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Tire pressure monitoring system"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVMHD","Compression-ignition Medium HDV - Multipurpose","SHBG2VOCVMHD-002","HBG-06","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"Harbinger Motors, Inc.","SHBG2VOCVMHD","Compression-ignition Medium HDV - Multipurpose","SHBG2VOCVMHD-002","HBG-06","Electricity","10 years / 185,000 mi","Y","N",246,0,0,"Vocational BEV delivery van","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Tire pressure monitoring system"]
[2025,"ENVIROTECH DRIVE SYSTEMS INC","SETD2VOCVEVT","Compression-ignition Light HDV - Urban","SETD2VOCVEVT-001","C Series Cutaway","Electricity","15 years / 150,000 mi","Y","N",385,0,0,"Phase 2 GHG LHD Vehicle Family. The Urban Cab Over is a battery-electric Class 4-5 cab chassis and will be built as an incomplete vehicle for sale to final manufacturers. The C Series Logistic is a complete battery-electric Class 4 delivery van. The C Series Cutaway is an incomplete battery-electric Class 4 cutaway chassis that will be offered for sale to final manufacturers.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"ENVIROTECH DRIVE SYSTEMS INC","SETD2VOCVEVT","Compression-ignition Light HDV - Urban","SETD2VOCVEVT-001","Urban Cab Over","Electricity","15 years / 150,000 mi","Y","N",385,0,0,"Phase 2 GHG LHD Vehicle Family. The Urban Cab Over is a battery-electric Class 4-5 cab chassis and will be built as an incomplete vehicle for sale to final manufacturers. The C Series Logistic is a complete battery-electric Class 4 delivery van. The C Series Cutaway is an incomplete battery-electric Class 4 cutaway chassis that will be offered for sale to final manufacturers.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"ENVIROTECH DRIVE SYSTEMS INC","SETD2VOCVEVT","Compression-ignition Light HDV - Urban","SETD2VOCVEVT-001","C Series Logistic","Electricity","15 years / 150,000 mi","Y","N",385,0,0,"Phase 2 GHG LHD Vehicle Family. The Urban Cab Over is a battery-electric Class 4-5 cab chassis and will be built as an incomplete vehicle for sale to final manufacturers. The C Series Logistic is a complete battery-electric Class 4 delivery van. The C Series Cutaway is an incomplete battery-electric Class 4 cutaway chassis that will be offered for sale to final manufacturers.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Low rolling resistance tires (all)"]
[2025,"SEA Electric","SSEE2VOCVSEA","Compression-ignition Light HDV - Multipurpose","SSEE2VOCVSEA-001","Make: SEA; Model: 5e","Electricity","15 years / 150,000 mi","Y","N",344,0,0,"Family includes Class 5 vocational vehicles with battery electric powered traction motors. Primarily short range intra city, urban operation.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FD5000GL","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FD4000","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FD6000MS","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FDB7000","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FD3000","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FDB5000","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FDC400S","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FDB4000","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"Terex Corporation","STRX2VOCVLRR","Concrete mixer","STRX2VOCVLRR-001","FDC300S","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Phase 2 GHG Heavy HDV Family. Class 8 diesel-powered front discharge concrete mixer trucks.","Y",0,1,"N","N",{"$nulls":14},"Y","2024-11-01","Low rolling resistance tires (steer)"]
[2025,"The Lion Electric Co USA","SLEL2VOCVLD1","School bus","SLEL2VOCVLD1-002","LIOND","Electricity","10 years / 185,000 mi","N","N",291,0,0,"TYPE D SCHOOL BUS UP TO 84 PASSENGERS","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-05-24","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"Newell Coach Corporation","RNCC2VOCVXEC","Motor home","RNCC2VOCVXEC-001-R01","Newell P50","Diesel","10 years / 185,000 mi","N","N",{"$nulls":3},"Motor Home","Y",0,1,"N","N",{"$nulls":14},"Y","2024-07-16","Low rolling resistance tires (all)"]
[2024,"Newell Coach Corporation","RNCC2VOCVXEC","Motor home","RNCC2VOCVXEC-001-R01","Newell P50","Diesel","10 years / 185,000 mi","N","N",{"$nulls":3},"Motor Home","Y",0,1,"N","N",{"$nulls":14},"Y","2024-07-16","Tire pressure monitoring system"]
[2024,"Global Environmental Product Inc","RGE12VOCVS4E","Refuse hauler","RGE12VOCVS4E-002","HSDE","Electricity","10 years / 435,000 mi","N","N",313,0,0,"A street sweeping vehicle use to pick up refuse on the road and load it into a hopper. Then transport the waste to the cities local waste facility.","Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-08","Vehicle speed limiter"]
[2024,"Global Environmental Product Inc","RGE12VOCVS4E","Refuse hauler","RGE12VOCVS4E-002","NYCE","Electricity","10 years / 435,000 mi","N","N",313,0,0,"A street sweeping vehicle use to pick up refuse on the road and load it into a hopper. Then transport the waste to the cities local waste facility.","Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-08","Vehicle speed limiter"]
[2024,"Global Environmental Product Inc","RGE12VOCVS4E","Refuse hauler","RGE12VOCVS4E-002","R4E","Electricity","10 years / 435,000 mi","N","N",313,0,0,"A street sweeping vehicle use to pick up refuse on the road and load it into a hopper. Then transport the waste to the cities local waste facility.","Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-08","Vehicle speed limiter"]
[2024,"Global Environmental Product Inc","RGE12VOCVS4E","Refuse hauler","RGE12VOCVS4E-002","M4E","Electricity","10 years / 435,000 mi","N","N",313,0,0,"A street sweeping vehicle use to pick up refuse on the road and load it into a hopper. Then transport the waste to the cities local waste facility.","Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-08","Vehicle speed limiter"]
[2024,"Dennis Eagle Inc","RDEI2VOCVDEI","Mixed-use vehicle","RDEI2VOCVDEI-002","DENNIS EAGLE, INC.","Compressed Natural Gas","10 years / 435,000 mi","N","N",319,285,309,"Dennis Eagle application for carryover MY2023 vehicle family PDEI2VOCVDEI that is a Mixed-Use vehicle used as a vocational road striper vehicle.","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-10-30","Low rolling resistance tires (all)"]
[2024,"Dennis Eagle Inc","RDEI2VOCVDEI","Mixed-use vehicle","RDEI2VOCVDEI-002","DENNIS EAGLE, INC.","Diesel","10 years / 435,000 mi","N","N",319,285,309,"Dennis Eagle application for carryover MY2023 vehicle family PDEI2VOCVDEI that is a Mixed-Use vehicle used as a vocational road striper vehicle.","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-10-30","Low rolling resistance tires (all)"]
[2024,"Dennis Eagle Inc","RDEI2VOCVDIE","Refuse hauler","RDEI2VOCVDIE-001","DENNIS EAGLE, INC.","Compressed Natural Gas","10 years / 435,000 mi","N","N",313,285,309,"HDD Vocational Custom Chassis Carryover Application for vehicle certification as use as a refuse hauler.","Y",0,1,"Y","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-10-30","Low rolling resistance tires (all)"]
[2024,"Dennis Eagle Inc","RDEI2VOCVDIE","Refuse hauler","RDEI2VOCVDIE-001","DENNIS EAGLE, INC.","Diesel","10 years / 435,000 mi","N","N",313,285,309,"HDD Vocational Custom Chassis Carryover Application for vehicle certification as use as a refuse hauler.","Y",0,1,"Y","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-10-30","Low rolling resistance tires (all)"]
[2024,"CENNTRO AUTOMOTIVE CORPORATION","RCAC2VOCV450","Compression-ignition Light HDV - Multipurpose","RCAC2VOCV450-001-R01","Logistar-LS450","Electricity","15 years / 150,000 mi","N","N",344,0,0,"Urban/Suburban Delivery and Service, Landscape, Plumbing, Electrician, and so forth.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-01-03","Low rolling resistance tires (all)"]
[2024,"CENNTRO AUTOMOTIVE CORPORATION","RCAC2VOCV450","Compression-ignition Light HDV - Multipurpose","RCAC2VOCV450-001-R01","Logistar-LS450","Electricity","15 years / 150,000 mi","N","N",344,0,0,"Urban/Suburban Delivery and Service, Landscape, Plumbing, Electrician, and so forth.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-01-03","Tire pressure monitoring system"]
[2024,"FCA US LLC","RCRX2VOCV067","Compression-ignition Light HDV - Multipurpose","RCRX2VOCV067-001","RAM 5500 Cab Chassis, RAM 4500 Cab Chassis, RAM 3500 Cab Chassis","Diesel","15 years / 150,000 mi","Y","N",344,314,353,"Cab chassis vehicles assembly by FCA US LLC with engines supplied by Cummins and transmissions supplied by AISIN.","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2024-11-15","Low rolling resistance tires (drive)"]
[2024,"FCA US LLC","RCRX2VOCV067","Compression-ignition Light HDV - Multipurpose","RCRX2VOCV067-001","RAM 5500 Cab Chassis, RAM 4500 Cab Chassis, RAM 3500 Cab Chassis","Diesel","15 years / 150,000 mi","Y","N",344,314,353,"Cab chassis vehicles assembly by FCA US LLC with engines supplied by Cummins and transmissions supplied by AISIN.","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2024-11-15","Low rolling resistance tires (steer)"]
[2024,"FCA US LLC","RCRX2VOCV067","Compression-ignition Light HDV - Multipurpose","RCRX2VOCV067-001","RAM 5500 Cab Chassis, RAM 4500 Cab Chassis, RAM 3500 Cab Chassis","Diesel","15 years / 150,000 mi","Y","N",344,314,353,"Cab chassis vehicles assembly by FCA US LLC with engines supplied by Cummins and transmissions supplied by AISIN.","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2024-11-15","Low rolling resistance tires (all)"]
[2024,"Tesla, Inc.","RTSL2TRACSEE","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RTSL2TRACSEE-002","Tesla Semi Long Range","Electricity","10 years / 435,000 mi","Y","N",80.4,0,0,null,"Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-10-09","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2024,"E-ONE, INC.","RENE2VOCV001","Emergency vehicle","RENE2VOCV001-001","Rescue","Diesel","10 years / 435,000 mi","Y","N",324,301,320,"This family is made up of standard pumper, aerial, and rescue trucks used in the fire and emergency industry.","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"E-ONE, INC.","RENE2VOCV001","Emergency vehicle","RENE2VOCV001-001","Pumper","Diesel","10 years / 435,000 mi","Y","N",324,301,320,"This family is made up of standard pumper, aerial, and rescue trucks used in the fire and emergency industry.","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"E-ONE, INC.","RENE2VOCV001","Emergency vehicle","RENE2VOCV001-001","Aerial","Diesel","10 years / 435,000 mi","Y","N",324,301,320,"This family is made up of standard pumper, aerial, and rescue trucks used in the fire and emergency industry.","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 389","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","L770","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W990","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T170","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 348","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 589","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T380","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T800","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 337","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","L770","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,"\"Adding following  Engine families to all engine powered vehicle families. No changes in vehicle design / architecture, GEM parameters, FEL\"","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","T880","Compressed Natural Gas","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","RPCR2VOCVC6R-028","Model 220","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","RPCR2VOCVC6R-028","Model 330","Compressed Natural Gas","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","RPCR2VOCVC5R-027","T680","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","RPCR2VOCVC5R-027","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","RPCR2VOCVC5R-027","T440","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","RPCR2VOCVC4R-026","Model 389","Diesel","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","RPCR2VOCVC4R-026","T480","Compressed Natural Gas","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","RPCR2VOCVC6K-025","T800","Diesel","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","RPCR2VOCVC6K-025","K370","Diesel","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCE2-005","Model 220","Diesel","10 years / 435,000 mi","Y","N",80.9,57.2,164.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCE2-005","Model 536","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.9,57.2,164.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCE2-005","T470","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.9,57.2,164.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","RPCR2VOCVC6K-025","T480","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","RPCR2VOCVC6K-025","Model 389","Compressed Natural Gas","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","RPCR2VOCVC5K-024","Model 548","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","RPCR2VOCVC5K-024","Model 330","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","RPCR2VOCVC5K-024","Model 520","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","RPCR2VOCVC4K-023","K370","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","RPCR2VOCVC4K-023","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","RPCR2VOCVC4K-023","T440","Diesel","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RPCR2TRACCX8-011","Model 348","Diesel","10 years / 435,000 mi","Y","N",50.2,34,105,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RPCR2TRACCX8-011","T800","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",50.2,34,105,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","RPCR2TRACCW7-016","Model 579","Compressed Natural Gas","10 years / 435,000 mi","Y","N",44.5,27,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCF2-006","T680","Diesel","10 years / 435,000 mi","Y","N",76.2,57.4,165.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCF2-006","T480","Diesel","10 years / 435,000 mi","Y","N",76.2,57.4,165.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCF2-006","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",76.2,57.4,165.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","RPCR2TRACCW7-016","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",44.5,27,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","RPCR2TRACCW7-016","Model 365","Diesel","10 years / 435,000 mi","Y","N",44.5,27,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","RPCR2TRACCV7-015","Model 567","Diesel","10 years / 435,000 mi","Y","N",46.9,26.900000000000002,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","RPCR2TRACCV7-015","Model 567","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",46.9,26.900000000000002,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","RPCR2TRACCV7-015","T800","Diesel","10 years / 435,000 mi","Y","N",46.9,26.900000000000002,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","RPCR2TRACCU7-014","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",44.2,27.2,113.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","RPCR2TRACCU7-014","Model 389","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",44.2,27.2,113.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Expiring engine shutoff"]
[2024,"PACCAR Inc","RPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","RPCR2TRACCT6-013","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",50.800000000000004,33.7,109.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","RPCR2TRACCT6-013","Model 520","Diesel","10 years / 435,000 mi","Y","N",50.800000000000004,33.7,109.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","RPCR2TRACCT6-013","Model 389","Compressed Natural Gas","10 years / 435,000 mi","Y","N",50.800000000000004,33.7,109.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","RPCR2TRACCS6-010","T880","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.800000000000004,33.6,109.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","RPCR2TRACCS6-010","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.800000000000004,33.6,109.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","RPCR2TRACCS6-010","L770","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.800000000000004,33.6,109.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","RPCR2TRACCR6-012","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.4,34,110.2,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","RPCR2TRACCR6-012","Model 535","Diesel","10 years / 435,000 mi","Y","N",51.4,34,110.2,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","RPCR2TRACCR6-012","Model 536","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.4,34,110.2,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCJ3-009","Model 367","Compressed Natural Gas","10 years / 435,000 mi","Y","N",68,45.800000000000004,170.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Expiring engine shutoff"]
[2024,"PACCAR Inc","RPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCJ3-009","Model 365","Diesel","10 years / 435,000 mi","Y","N",68,45.800000000000004,170.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCJ3-009","T370","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",68,45.800000000000004,170.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCJ3-009","T480","Diesel","10 years / 435,000 mi","Y","N",68,45.800000000000004,170.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCH3-008","T480","Diesel","10 years / 435,000 mi","Y","N",73.5,45.7,170.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCH3-008","T880","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",73.5,45.7,170.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCH3-008","C500","Diesel","10 years / 435,000 mi","Y","N",73.5,45.7,170.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCG3-007","T440","Diesel","10 years / 435,000 mi","Y","N",70.7,46.800000000000004,174,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCG3-007","C500","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",70.7,46.800000000000004,174,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCG3-007","T480","Compressed Natural Gas","10 years / 435,000 mi","Y","N",70.7,46.800000000000004,174,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","W900","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","T800","Diesel","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","T370","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","T470","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"New Flyer of America Inc.","RNFA2VOCVENH","Transit and other bus","RNFA2VOCVENH-005-R01","New Flyer XDE35","Diesel","10 years / 435,000 mi","Y","N",300,264,322,"Diesel, Diesel-Electric, and CNG Powered Heavy Duty Urban Transit Bus","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","N","N","N","2024-01-01","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","RPCR2VOCVC2K-018","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","RPCR2VOCVC2K-018","Model 567","Diesel","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","RPCR2VOCVC2K-018","K370","Diesel","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","RPCR2VOCVC3R-022","Model 536","Compressed Natural Gas","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","RPCR2VOCVC3R-022","Model 348","Diesel","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","RPCR2VOCVC2R-021","Model 220","Diesel","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","RPCR2VOCVC2R-021","Model 567","Diesel","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","RPCR2VOCVC2R-021","L770","Compressed Natural Gas","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","RPCR2VOCVC1R-020","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","RPCR2VOCVC1R-020","T800","Diesel","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","RPCR2VOCVC1R-020","W900","Diesel","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","RPCR2VOCVC3K-019","Model 535","Diesel","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","RPCR2VOCVC3K-019","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","RPCR2VOCVC3K-019","Model 537","Compressed Natural Gas","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","RPCR2VOCVC1K-017","T370","Compressed Natural Gas","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","RPCR2VOCVC1K-017","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","RPCR2VOCVC1K-017","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 579","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 367","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVL00","Compression-ignition Heavy HDV - Urban","RVPT2VOCVL00-029-R01","Mack Granite (AF, AB)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",283,239,367,"URBAN DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Vehicle speed limiter"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVM00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVM00-030","Volvo VNL","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,182,356,"MULTI-PURPOSE DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Aerodynamic roof fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRACW00","Class 8 heavy-haul high-roof day cab tractor","RVPT2TRACW00-014-R01","MACK ANTHEM","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.4,41.1,66.8,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Aerodynamic roof fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRACX00","Class 8 heavy-haul low-roof sleeper cab tractor","RVPT2TRACX00-002-R01","MACK ANTHEM","Diesel","10 years / 435,000 mi","Y","N",44.5,30.7,61.300000000000004,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Tire pressure monitoring system"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRACZ00","Class 8 heavy-haul high-roof sleeper cab tractor","RVPT2TRACZ00-004-R01","VOLVO VNR","Compressed Natural Gas","10 years / 435,000 mi","Y","N",44.2,32.3,62,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVH00","Compression-ignition Heavy HDV - Urban","RVPT2VOCVH00-024-R01","Volvo New VNL","Compressed Natural Gas","10 years / 435,000 mi","Y","N",283,242,360,"URBAN DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS, ELECTRIC VEHICLES","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Automatic engine shutdown system"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRACT00","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RVPT2TRACT00-011-R01","Volvo NEW VNL","Compressed Natural Gas","10 years / 435,000 mi","Y","N",73.5,54.6,113.10000000000001,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Automatic engine shutdown system"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRACQ00","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RVPT2TRACQ00-008-R02","MACK ANTHEM","Diesel","10 years / 435,000 mi","Y","N",76.2,62.4,117.7,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRAC100","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RVPT2TRAC100-006-R01","Volvo VNL (New VNL)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",76.2,62.4,117.7,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please see AES Document: \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please see AES Document: \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV04U","Compression-ignition Medium HDV - Urban","RDTN2VOCV04U-038","FCCC XBA/XBP/XBR/XBS Chassis","Compressed Natural Gas","10 years / 185,000 mi","Y","N",271,227,442,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV04R","Compression-ignition Medium HDV - Regional","RDTN2VOCV04R-037","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",221,181,327,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV16U","Compression-ignition Medium HDV - Urban","RDTN2VOCV16U-053","Freightliner SD108/SD114/SD122","Diesel","10 years / 185,000 mi","Y","N",271,227,442,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRAC800","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RVPT2TRAC800-018","Volvo VNL","Diesel","10 years / 435,000 mi","Y","N",73.5,54.6,113.10000000000001,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Aerodynamic roof fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRAC300","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RVPT2TRAC300-005-R01","Mack Pinnacle PI (CHU)","Diesel","10 years / 435,000 mi","Y","N",80.4,65.3,119.8,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please see AES Document: \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please see AES Document: \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"International Motors, LLC","RNVX2VOCVXNM","Compression-ignition Class 7 Vocational Tractor - Multipurpose","RNVX2VOCVXNM-018","HV","Diesel","10 years / 185,000 mi","Y","N",246,205,354,"Heavy Hauler Tractor, On/Off Highway Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"International Motors, LLC","RNVX2TRACXMS","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RNVX2TRACXMS-039","RH","Diesel","10 years / 435,000 mi","Y","N",70.7,61,119.2,"Tractor","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"e-Roll Corporation","RERL2VOCV008","Compression-ignition Medium HDV - Multipurpose","RERL2VOCV008-002","SH5140SCEV","Electricity","10 years / 185,000 mi","N","N",246,0,0,"Both vehicles are 100% Pure Electric Pupil Transportation Buses *(School Buses), designed specifically for the transportation of school-aged children.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-03-01","Vehicle includes other advanced-technology components (i.e., non-hybrid system)"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVJ00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVJ00-025","Volvo VN(R,L)","Diesel","10 years / 435,000 mi","Y","N",242,205,361,"Multi-Purpose DISTRIBUTION, DUMP TRUCKS, REFUSE,  DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVH10","Compression-ignition Heavy HDV - Urban","RVPT2VOCVH10-026","Mack LRe","Electricity","10 years / 435,000 mi","Y","N",283,0,0,"URBAN DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC12C","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RDTN2TRAC12C-008","Western Star 47X/49X/57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",73.5,62.9,116.3,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Refuse Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","N","Y","2024-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RDTN2TRAC10C-006","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",68,58.7,118.3,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RDTN2TRAC07C-003","Freightliner Cascadia 116/126","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,99.5,170.6,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Aerodynamic roof fairing"]
[2024,"International Motors, LLC","RNVX2TRACXJS","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RNVX2TRACXJS-035","LS","Diesel","10 years / 435,000 mi","Y","N",80.4,72.4,124.9,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"International Motors, LLC","RNVX2TRACXHU","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RNVX2TRACXHU-033","LT","Diesel","10 years / 435,000 mi","Y","N",50.2,44,73.2,"Tractor","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2024-01-01","Adjustable height aerodynamic roof fairing"]
[2024,"International Motors, LLC","RNVX2TRACXFH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RNVX2TRACXFH-024","LT","Diesel","10 years / 185,000 mi","Y","N",106.60000000000001,88.9,162.4,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRAC800","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RVPT2TRAC800-018","Volvo VNL","Diesel","10 years / 435,000 mi","Y","N",73.5,54.6,113.10000000000001,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Automatic engine shutdown system"]
[2024,"International Motors, LLC","RNVX2TRACXLA","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RNVX2TRACXLA-048","LT","Diesel","10 years / 435,000 mi","Y","N",73.5,62.6,116.7,"Tractor","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC33E","Class 8 heavy-haul high-roof day cab tractor","RDTN2TRAC33E-024","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.4,45.1,71.60000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2024-01-01","Automatic tire inflation system"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC30E","Class 8 heavy-haul low-roof sleeper cab tractor","RDTN2TRAC30E-021","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",44.5,38.4,68.4,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC14E","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RDTN2TRAC14E-019","Western Star 47X/49X/57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",70.7,61,116.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC11E","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RDTN2TRAC11E-016","Western Star 47X/49X/57X","Diesel","10 years / 435,000 mi","Y","N",80.9,76.2,128.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"International Motors, LLC","RNVX2TRACXFH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RNVX2TRACXFH-024","RH","Diesel","10 years / 185,000 mi","Y","N",106.60000000000001,88.9,162.4,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"International Motors, LLC","RNVX2VOCVXBM","Compression-ignition Medium HDV - Multipurpose","RNVX2VOCVXBM-005","MV","Diesel","10 years / 185,000 mi","Y","N",246,205,354,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (all)"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV04M","Compression-ignition Medium HDV - Multipurpose","RDTN2VOCV04M-036","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",246,203,403,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVM00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVM00-030","Mack Anthem AN(AB)","Diesel","10 years / 435,000 mi","Y","N",242,182,356,"MULTI-PURPOSE DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (all)"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVJ00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVJ00-025","Mack TerraPro (LR, MR)","Diesel","10 years / 435,000 mi","Y","N",242,205,361,"Multi-Purpose DISTRIBUTION, DUMP TRUCKS, REFUSE,  DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Engine shutoff after 5 minutes or less of idling"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV04A","Compression-ignition Medium HDV - Urban","RDTN2VOCV04A-069","FCCC MT50e Chassis","Electricity","10 years / 185,000 mi","Y","N",271,0,0,"City Transit Bus Pickup and Delivery School and Transit Bus Utility/Repair/Maintenance Service","N",null,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC09E","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RDTN2TRAC09E-014","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",76.2,68.60000000000001,118.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Aerodynamic roof fairing"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC08E","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RDTN2TRAC08E-013","Freightliner Cascadia 116/126","Diesel","10 years / 185,000 mi","Y","N",106.60000000000001,97.8,167.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"Daimler Truck North America LLC","RDTN2TRACHHC","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RDTN2TRACHHC-026","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",50.2,44.800000000000004,79.2,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2024-01-01","Tire pressure monitoring system"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC34C","Class 8 heavy-haul high-roof sleeper cab tractor","RDTN2TRAC34C-032","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 435,000 mi","Y","N",44.2,37.1,69.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2024-01-01","Low rolling resistance tires (all)"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC30C","Class 8 heavy-haul low-roof sleeper cab tractor","RDTN2TRAC30C-028","Western Star 47X/49X/57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",44.5,38.4,68.4,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2024-01-01","Gap reducing fairing"]
[2024,"Daimler Truck North America LLC","RDTN2TRAC30C","Class 8 heavy-haul low-roof sleeper cab tractor","RDTN2TRAC30C-028","Freightliner SD108/SD114/SD122","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",44.5,38.4,68.4,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2024-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"International Motors, LLC","RNVX2TRACXHU","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RNVX2TRACXHU-033","RH","Diesel","10 years / 435,000 mi","Y","N",50.2,44,73.2,"Tractor","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2024-01-01","Engine shutoff after 5 minutes or less of idling"]
[2024,"International Motors, LLC","RNVX2TRACXJW","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RNVX2TRACXJW-029","LT","Diesel","10 years / 435,000 mi","Y","N",80.4,72.4,124.9,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRAC110","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RVPT2TRAC110-015","Volvo VNRe","Electricity","10 years / 435,000 mi","Y","N",76.2,0,0,"BULK HAUL, REGIONAL HAUL","Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","N","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV05V","Compression-ignition Heavy HDV - Urban","RDTN2VOCV05V-051","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Compressed Natural Gas","10 years / 435,000 mi","Y","N",283,231,376,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV05N","Compression-ignition Heavy HDV - Multipurpose","RDTN2VOCV05N-042","FCCC XBA/XBP/XBR/XBS Chassis","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",242,205,349,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV04S","Compression-ignition Medium HDV - Regional","RDTN2VOCV04S-047","FCCC S2, S2C, S2G, S2RV","Diesel","10 years / 185,000 mi","Y","N",221,181,327,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Daimler Truck North America LLC","RDTN2VOCV04N","Compression-ignition Medium HDV - Multipurpose","RDTN2VOCV04N-039","Freightliner SD108/SD114/SD122","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",246,203,403,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVK00","Compression-ignition Heavy HDV - Regional","RVPT2VOCVK00-028-R01","Mack LR","Diesel","10 years / 435,000 mi","Y","N",194,146,278,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Gap reducing fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVK00","Compression-ignition Heavy HDV - Regional","RVPT2VOCVK00-028-R01","Volvo VAH (AF,AB)","Diesel","10 years / 435,000 mi","Y","N",194,146,278,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"International Motors, LLC","RNVX2TRACXJS","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RNVX2TRACXJS-035","LT","Diesel","10 years / 435,000 mi","Y","N",80.4,72.4,124.9,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (steer)"]
[2024,"International Motors, LLC","RNVX2TRACXHS","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RNVX2TRACXHS-034","LT","Diesel","10 years / 435,000 mi","Y","N",80.9,68.1,120.8,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Adjustable height aerodynamic roof fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVM00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVM00-030","Volvo VNL","Diesel","10 years / 435,000 mi","Y","N",242,182,356,"MULTI-PURPOSE DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVJ00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVJ00-025","Mack TerraPro (LR, MR)","Diesel","10 years / 435,000 mi","Y","N",242,205,361,"Multi-Purpose DISTRIBUTION, DUMP TRUCKS, REFUSE,  DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCH3-008","Model 520","Diesel","10 years / 435,000 mi","Y","N",73.5,45.7,170.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Automatic engine shutdown system"]
[2024,"PACCAR Inc","RPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCH3-008","T380","Diesel","10 years / 435,000 mi","Y","N",73.5,45.7,170.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCH3-008","Model 367","Diesel","10 years / 435,000 mi","Y","N",73.5,45.7,170.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Automatic engine shutdown system"]
[2024,"PACCAR Inc","RPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCH3-008","T480","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",73.5,45.7,170.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCJ3-009","W990","Compressed Natural Gas","10 years / 435,000 mi","Y","N",68,45.800000000000004,170.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCJ3-009","Model 579","Diesel","10 years / 435,000 mi","Y","N",68,45.800000000000004,170.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCJ3-009","T440","Diesel","10 years / 435,000 mi","Y","N",68,45.800000000000004,170.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCG3-007","T470","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",70.7,46.800000000000004,174,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCG3-007","Model 589","Compressed Natural Gas","10 years / 435,000 mi","Y","N",70.7,46.800000000000004,174,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","RPCR2TRACCG3-007","T380","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",70.7,46.800000000000004,174,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","RPCR2VOCVC6R-028","Model 220","Diesel","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","RPCR2VOCVC6R-028","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","RPCR2VOCVC6R-028","T800","Diesel","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","RPCR2VOCVC5R-027","T380","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","RPCR2VOCVC5R-027","W900","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","RPCR2VOCVC4R-026","T470","Diesel","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","RPCR2VOCVC4R-026","Model 536","Diesel","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","RPCR2VOCVC4R-026","Model 589","Compressed Natural Gas","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","RPCR2VOCVC3R-022","Model 330","Diesel","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","RPCR2VOCVC3R-022","T440","Diesel","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","RPCR2VOCVC3R-022","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","RPCR2VOCVC2R-021","Model 548","Compressed Natural Gas","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","RPCR2VOCVC2R-021","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","RPCR2VOCVC2R-021","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","RPCR2TRACCR6-012","Model 367","Diesel","10 years / 435,000 mi","Y","N",51.4,34,110.2,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","RPCR2TRACCR6-012","W900","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.4,34,110.2,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRACN00","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RVPT2TRACN00-020","Volvo VNR","Diesel","10 years / 435,000 mi","Y","N",50.2,40.6,66.9,"Heavy Haul Applications.","Y",0,1,"N","N","Y",null,"Please see submitted document \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please see submitted document \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Gap reducing fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRAC800","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RVPT2TRAC800-018","Volvo VNR","Diesel","10 years / 435,000 mi","Y","N",73.5,54.6,113.10000000000001,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Automatic engine shutdown system"]
[2024,"PACCAR Inc","RPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","RPCR2TRACCS6-010","Model 330","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.800000000000004,33.6,109.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","RPCR2TRACCS6-010","Model 535","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.800000000000004,33.6,109.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2TRACT00","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","RVPT2TRACT00-011-R01","VOLVO VNR","Compressed Natural Gas","10 years / 435,000 mi","Y","N",73.5,54.6,113.10000000000001,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_RVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2024-01-01","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACEF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACEF2-030","Model 579","Electricity","10 years / 435,000 mi","Y","N",76.2,0,0,null,"Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2024-01-01","Expiring vehicle speed limiter"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVM00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVM00-030","Volvo VAH (AF,AB)","Diesel","10 years / 435,000 mi","Y","N",242,182,356,"MULTI-PURPOSE DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Vehicle speed limiter"]
[2024,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","RVPT2VOCVJ00","Compression-ignition Heavy HDV - Multipurpose","RVPT2VOCVJ00-025","Volvo New VNL","Diesel","10 years / 435,000 mi","Y","N",242,205,361,"Multi-Purpose DISTRIBUTION, DUMP TRUCKS, REFUSE,  DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-01-01","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","RPCR2VOCVC3K-019","T480","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","RPCR2VOCVC3K-019","T280","Diesel","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","RPCR2VOCVC3K-019","W990","Compressed Natural Gas","10 years / 185,000 mi","Y","N",271,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","RPCR2VOCVC1K-017","Model 537","Compressed Natural Gas","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","RPCR2VOCVC1K-017","Model 536","Diesel","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","RPCR2VOCVC1K-017","T800","Compressed Natural Gas","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RPCR2TRACCX8-011","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",50.2,34,105,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RPCR2TRACCX8-011","Model 537","Diesel","10 years / 435,000 mi","Y","N",50.2,34,105,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","RPCR2TRACCX8-011","T880","Compressed Natural Gas","10 years / 435,000 mi","Y","N",50.2,34,105,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","RPCR2VOCVC5K-024","W900","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","RPCR2VOCVC5K-024","C500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","RPCR2VOCVC5K-024","T480","Compressed Natural Gas","10 years / 435,000 mi","Y","N",242,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","RPCR2VOCVC4K-023","Model 337","Diesel","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","RPCR2VOCVC4K-023","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",194,200,458,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","RPCR2VOCVC6K-025","Model 579","Diesel","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","RPCR2VOCVC6K-025","Model 367","Compressed Natural Gas","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","RPCR2VOCVC6K-025","W990","Compressed Natural Gas","10 years / 435,000 mi","Y","N",283,200,508,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","RPCR2VOCVC1R-020","Model 589","Diesel","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","RPCR2VOCVC1R-020","Model 348","Diesel","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","RPCR2VOCVC1R-020","Model 337","Diesel","10 years / 185,000 mi","Y","N",221,227,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","RPCR2VOCVC2K-018","Model 337","Compressed Natural Gas","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","RPCR2VOCVC2K-018","Model 536","Compressed Natural Gas","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","RPCR2VOCVC2K-018","K370","Diesel","10 years / 185,000 mi","Y","N",246,212,614,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","RPCR2TRACCU7-014","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",44.2,27.2,113.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Expiring engine shutoff"]
[2024,"PACCAR Inc","RPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","RPCR2TRACCU7-014","T880","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",44.2,27.2,113.9,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Engine shutoff after 5 minutes or less of idling"]
[2024,"PACCAR Inc","RPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","RPCR2TRACCT6-013","Model 337","Compressed Natural Gas","10 years / 435,000 mi","Y","N",50.800000000000004,33.7,109.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","RPCR2TRACCT6-013","W900","Compressed Natural Gas","10 years / 435,000 mi","Y","N",50.800000000000004,33.7,109.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","RPCR2TRACCT6-013","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",50.800000000000004,33.7,109.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCE2-005","Model 520","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.9,57.2,164.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCE2-005","C500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.9,57.2,164.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCE2-005","T680","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.9,57.2,164.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCE2-005","T440","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.9,57.2,164.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","T880","Diesel","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Vehicle weight reduction"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","C500","Diesel","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","T680","Diesel","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCD2-004","Model 589","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",80.4,58.7,169,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","RPCR2TRACCW7-016","Model 389","Compressed Natural Gas","10 years / 435,000 mi","Y","N",44.5,27,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","RPCR2TRACCW7-016","W900","Diesel","10 years / 435,000 mi","Y","N",44.5,27,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","RPCR2TRACCV7-015","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,26.900000000000002,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Engine shutoff after 5 minutes or less of idling"]
[2024,"PACCAR Inc","RPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","RPCR2TRACCV7-015","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,26.900000000000002,112.7,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 589","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (all)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","W900","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (steer)"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","Model 579","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCC1-003","T170","Diesel","10 years / 185,000 mi","Y","N",99.8,74.60000000000001,213.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","T480","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 536","Diesel","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Expiring vehicle speed limiter"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 330","Compressed Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCB1-002","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",107.10000000000001,74.3,213.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic side skirt and/or fuel tank fairing"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","Model 589","Compressed Natural Gas","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","W900","Diesel","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Gap reducing fairing"]
[2024,"PACCAR Inc","RPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","RPCR2TRACCA1-001","Model 365","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",106.60000000000001,76.60000000000001,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Tire pressure monitoring system"]
[2024,"PACCAR Inc","RPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCF2-006","Model 348","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",76.2,57.4,165.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024,"PACCAR Inc","RPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCF2-006","Model 535","Diesel","10 years / 435,000 mi","Y","N",76.2,57.4,165.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Low rolling resistance tires (drive)"]
[2024,"PACCAR Inc","RPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","RPCR2TRACCF2-006","T370","Diesel","10 years / 435,000 mi","Y","N",76.2,57.4,165.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2024-08-27","Aerodynamic roof fairing"]
[2024," BYD Auto Industry Company Limited","RBYD2VOCVHRC","Compression-ignition Heavy HDV - Regional","RBYD2VOCVHRC-001","BYD Electric Double-decker Coach 35 Ft.","Electricity","10 years / 435,000 mi","Y","N",194,0,0,"Application for BYD Electric Coach 35 Ft., BYD Electric Double-decker Coach 35 Ft., BYD Electric Coach 40 Ft., BYD Electric Coach 45 Ft., and BYD Electric Double-decker Coach 45 Ft.","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2024-01-01","Low rolling resistance tires (all)"]
[2023,"Motor Coach Industries","PMCH2VOCVMCI","Coach bus","PMCH2VOCVMCI-001-R01","Motor Coach Industries D4505","Compressed Natural Gas","10 years / 435,000 mi","Y","N",210,202,224,"Motor coach, ISTV, Over the road bus, charter bus, commuter bus","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","N","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Terex Corporation","PTRX2VOCVLRR","Concrete mixer","PTRX2VOCVLRR-001-R01","Terex FDB6000","Diesel","10 years / 435,000 mi","N","N",{"$nulls":3},"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers.  All new Terex Concrete Mixers use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":14},"Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRAC800","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","PVPT2TRAC800-015-R03","Volvo VNL","Compressed Natural Gas","10 years / 435,000 mi","Y","N",78,56,113.10000000000001,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRAC900","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","PVPT2TRAC900-014-R03","Volvo VNL","Diesel","10 years / 435,000 mi","Y","N",75.7,55.6,115.2,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\".","N",null,null,"N",null,"Please refer document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\".",null,null,"Y","Y","N","Y","2023-01-01","Vehicle weight reduction"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2VOCVH00","Compression-ignition Heavy HDV - Urban","PVPT2VOCVH00-002-R03","Mack Anthem AN(AB)","Diesel","10 years / 435,000 mi","Y","N",308,0,369,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS, ELECTRIC VEHICLES","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRACT00","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","PVPT2TRACT00-020-R04","Mack Pinnacle PI (CHU)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",78,56,113.10000000000001,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2VOCVG00","Compression-ignition Heavy HDV - Regional","PVPT2VOCVG00-001-R03","Mack Granite (AF, AB)","Diesel","10 years / 435,000 mi","Y","N",205,0,234,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRACS00","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","PVPT2TRACS00-019-R04","Mack Pinnacle PI (CHU)","Diesel","10 years / 435,000 mi","Y","N",72.3,55.7,113.2,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2023-01-01","Vehicle speed limiter"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRACY00","Class 8 heavy-haul mid-roof sleeper cab tractor","PVPT2TRACY00-025-R02","Volvo VNL","Diesel","10 years / 435,000 mi","Y","N",49.6,42.7,64.1,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2023-01-01","Gap reducing fairing"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRACY00","Class 8 heavy-haul mid-roof sleeper cab tractor","PVPT2TRACY00-025-R02","Mack ANTHEM AN (CXU)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",49.6,42.7,64.1,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2023-01-01","Aerodynamic roof fairing"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2VOCVJ00","Compression-ignition Heavy HDV - Multipurpose","PVPT2VOCVJ00-003-R03","Volvo VN(R,L)","Diesel","10 years / 435,000 mi","Y","N",261,0,347,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRACR00","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PVPT2TRACR00-018-R04","Mack Anthem AN (CHX)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,70.8,118.5,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2VOCVL00","Compression-ignition Heavy HDV - Urban","PVPT2VOCVL00-005-R04","Mack Granite (AF, AB)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,242,369,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Vehicle weight reduction"]
[2023,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","PVPT2TRAC100","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","PVPT2TRAC100-009-R03","VOLVO VNL 300","Diesel","10 years / 435,000 mi","Y","N",80.5,63.7,116.10000000000001,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_PVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2023-01-01","Engine shutoff after 5 minutes or less of idling"]
[2023,"International Motors, LLC","PNVX2TRACXFH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PNVX2TRACXFH-007","RH","Diesel","10 years / 185,000 mi","Y","N",113.5,92,161.9,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Gap reducing fairing"]
[2023,"International Motors, LLC","PNVX2TRACXEM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PNVX2TRACXEM-006","LT","Diesel","10 years / 185,000 mi","Y","N",113.2,91.2,152.5,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2023,"Blue Bird Body Company","PBBB2VOCVAHD","Transit and other bus","PBBB2VOCVAHD-006","All American","Electricity","10 years / 435,000 mi","Y","N",300,0,0,"Bus, Other Bus","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","N","2023-09-22","Low rolling resistance tires (drive)"]
[2023,"International Motors, LLC","PNVX2TRACXHA","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PNVX2TRACXHA-045","RH","Diesel","10 years / 435,000 mi","Y","N",52.4,35.6,61.300000000000004,"Tractor","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2023-01-01","Gap reducing fairing"]
[2023,"International Motors, LLC","PNVX2TRACXJS","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PNVX2TRACXJS-022","LT","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,70.5,119.8,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Adjustable height aerodynamic roof fairing"]
[2023,"International Motors, LLC","PNVX2TRACXJW","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PNVX2TRACXJW-009","LT","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,70.5,119.8,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC11C","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","PDTN2TRAC11C-006","Western Star 47X/49X/57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,74.9,128.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC06C","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PDTN2TRAC06C-001","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,90.7,155.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Tire pressure monitoring system"]
[2023,"Battle Motors, Inc.","PCCA2VOCVMD1","Compression-ignition Medium HDV - Urban","PCCA2VOCVMD1-003","Battle Motors","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,284,326,"Refuse hauler, Package delivery, Street sweeper","N",0,null,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2023-02-01","Low rolling resistance tires (all)"]
[2023,"Daimler Truck North America LLC","PDTN2TRACHHC","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PDTN2TRACHHC-016","Freightliner SD108/SD114/SD122","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.4,44.7,79.2,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2023-01-01","Tire pressure monitoring system"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV17V","Compression-ignition Heavy HDV - Urban","PDTN2VOCV17V-050","Freightliner M2 106/112","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,233,373,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV05N","Compression-ignition Heavy HDV - Multipurpose","PDTN2VOCV05N-044","FCCC S2, S2C, S2G, S2RV","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,206,348,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Vehicle weight reduction"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV05V","Compression-ignition Heavy HDV - Urban","PDTN2VOCV05V-043","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",308,233,373,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Vehicle weight reduction"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV04S","Compression-ignition Medium HDV - Regional","PDTN2VOCV04S-040","Freightliner M2 106/112","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,183,328,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV03S","Compression-ignition Medium HDV - Regional","PDTN2VOCV03S-036","FCCC MBC/MC/MT45/MT55 Chassis","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,183,328,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV05U","Compression-ignition Heavy HDV - Urban","PDTN2VOCV05U-059","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,233,373,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC14C","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","PDTN2TRAC14C-009","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",75.7,61,117.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","N","Y","2023-01-01","Aerodynamic roof fairing"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC13C","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PDTN2TRAC13C-008","Western Star 47X/49X/57X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,71.7,133.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","PDTN2TRAC10C-005","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72.3,58.800000000000004,118.60000000000001,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"Nikola Corporation","PNKC2TRACHP1","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PNKC2TRACHP1-002","Nikola TRE","Hydrogen","10 years / 435,000 mi","Y","N",85.60000000000001,0,0,"The Nikola TRE FCEV will be used primarily as a line haul tractor.","N",0,null,"N","N","N",null,null,"N",null,null,"Y","Fuel Cell Vehicle",{"$nulls":3},"N","N","N","Y","2023-08-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2023,"International Motors, LLC","PNVX2TRACXHA","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PNVX2TRACXHA-045","RH","Diesel","10 years / 435,000 mi","Y","N",52.4,35.800000000000004,61.300000000000004,"Tractor","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2023-01-01","Adjustable height aerodynamic roof fairing"]
[2023,"International Motors, LLC","PNVX2TRACXHH","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PNVX2TRACXHH-042","LS","Diesel","10 years / 435,000 mi","Y","N",52.4,41.800000000000004,66.1,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC13E","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PDTN2TRAC13E-027","Freightliner M2 106/112","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,71.7,133.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2023-01-01","Aerodynamic roof fairing"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC11E","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","PDTN2TRAC11E-023","Western Star 47X/49X/57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,74.9,128.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC09E","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","PDTN2TRAC09E-021","Freightliner M2 106/112","Diesel","10 years / 435,000 mi","Y","N",80.5,68.5,118.60000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Vehicle weight reduction"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC08E","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PDTN2TRAC08E-020","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,97.5,167.6,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Gap reducing fairing"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC06E","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PDTN2TRAC06E-018","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,90.7,155.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Gap reducing fairing"]
[2023,"International Motors, LLC","PNVX2VOCVXAU","Compression-ignition Light HDV - Urban","PNVX2VOCVXAU-014","CV","Diesel","15 years / 150,000 mi","Y","N",424,363,486,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, RV, Step-Van, Wrecker","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC08C","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PDTN2TRAC08C-003","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,97.5,167.6,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"International Motors, LLC","PNVX2VOCVXPU","Class 8 Vocational Tractor - Urban","PNVX2VOCVXPU-029","HX","Diesel","10 years / 435,000 mi","Y","N",308,238,372,"Heavy Hauler Tractor, On/Off Highway Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV04U","Compression-ignition Medium HDV - Urban","PDTN2VOCV04U-056","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,226,440,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV03M","Compression-ignition Medium HDV - Multipurpose","PDTN2VOCV03M-052","Freightliner M2 106/112","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,202,402,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Daimler Truck North America LLC","PDTN2TRACHHE","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PDTN2TRACHHE-029","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",52.4,44.7,79.2,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2023-01-01","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","PPCR2VOCVC1R-023","Model 365","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,148,578,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","PPCR2VOCVC1R-023","Model 337","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,148,578,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","PPCR2VOCVC1R-023","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,148,578,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (all)"]
[2023,"PACCAR Inc","PPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCF2-006","W900","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,155.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCF2-006","T800","Diesel","10 years / 435,000 mi","Y","N",80.5,56.6,155.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC30C","Class 8 heavy-haul low-roof sleeper cab tractor","PDTN2TRAC30C-011","Western Star 47X/49X/57X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,37.7,69.10000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC34E","Class 8 heavy-haul high-roof sleeper cab tractor","PDTN2TRAC34E-035","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",46.9,37.1,70.3,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2023-01-01","Automatic tire inflation system"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC31E","Class 8 heavy-haul mid-roof day cab tractor","PDTN2TRAC31E-032","Western Star 47X/49X/57X","Diesel","10 years / 435,000 mi","Y","N",54.1,48.9,69.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2023-01-01","Aerodynamic roof fairing"]
[2023,"Daimler Truck North America LLC","PDTN2TRAC30E","Class 8 heavy-haul low-roof sleeper cab tractor","PDTN2TRAC30E-031","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,37.7,69.10000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name Automatic Engine Shutdown for Tractors with DETROIT Engines",null,null,"Y","Y","Y","Y","2023-01-01","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","PPCR2TRACCS6-011","Model 579","Diesel","10 years / 435,000 mi","Y","N",54.1,33.5,110.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","PPCR2TRACCS6-011","C500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.5,110.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","PPCR2VOCVC6R-028","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,204,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","PPCR2VOCVC6R-028","Model 220","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,204,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","PPCR2VOCVC6R-028","Model 365","Diesel","10 years / 435,000 mi","Y","N",308,204,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","PPCR2VOCVC5K-021","T680","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,172,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","PPCR2VOCVC5K-021","Model 330","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,172,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","PPCR2VOCVC5R-027","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,172,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","PPCR2VOCVC5R-027","T440","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,172,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","PPCR2VOCVC5R-027","T380","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,172,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (all)"]
[2023,"PACCAR Inc","PPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","PPCR2VOCVC6K-022","Model 535","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,204,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","PPCR2VOCVC6K-022","T370","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,204,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","PPCR2VOCVC6K-022","Model 337","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,204,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","PPCR2VOCVC4K-020","Model 220","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,135,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","PPCR2VOCVC4K-020","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,135,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","PPCR2VOCVC4R-026","Model 220","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,135,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","PPCR2VOCVC4R-026","T470","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,135,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","PPCR2VOCVC4R-026","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,135,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","PPCR2VOCVC2R-024","T680","Diesel","10 years / 185,000 mi","Y","N",265,179,630,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","PPCR2VOCVC2R-024","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",265,179,630,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","PPCR2VOCVC3K-019","Model 330","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",296,216,618,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","PPCR2VOCVC3K-019","T270","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,216,618,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (all)"]
[2023,"PACCAR Inc","PPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","PPCR2TRACCT6-012","W990","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,110.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","PPCR2TRACCT6-012","Model 535","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,110.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Gap reducing fairing"]
[2023,"PACCAR Inc","PPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","PPCR2TRACCT6-012","T880","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,110.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","PPCR2VOCVC3K-019","T470","Diesel","10 years / 185,000 mi","Y","N",296,216,618,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","PPCR2VOCVC3R-025","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,216,618,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (all)"]
[2023,"PACCAR Inc","PPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","PPCR2VOCVC3R-025","Model 365","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,216,618,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","PPCR2VOCVC3R-025","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",296,216,618,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","PPCR2VOCVC2K-017","T370","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,179,630,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","PPCR2VOCVC2K-017","Model 579","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",265,179,630,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","PPCR2VOCVC2K-017","T480","Diesel","10 years / 185,000 mi","Y","N",265,179,630,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","PPCR2VOCVC1K-018","L770","Diesel","10 years / 185,000 mi","Y","N",234,148,578,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","PPCR2VOCVC1K-018","Model 325","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,148,578,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (all)"]
[2023,"PACCAR Inc","PPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","PPCR2VOCVC1K-018","Model 220","Diesel","10 years / 185,000 mi","Y","N",234,148,578,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","PPCR2TRACCW7-015","W900","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","PPCR2TRACCW7-015","Model 567","Diesel","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","PPCR2TRACCV7-014","Model 579","Diesel","10 years / 435,000 mi","Y","N",47.9,27.1,114.10000000000001,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","PPCR2TRACCV7-014","T680","Diesel","10 years / 435,000 mi","Y","N",47.9,27.1,114.10000000000001,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Gap reducing fairing"]
[2023,"PACCAR Inc","PPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","PPCR2TRACCU7-013","T680","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","PPCR2TRACCU7-013","Model 579","Diesel","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCJ3-009","Model 520","Diesel","10 years / 435,000 mi","Y","N",72.3,45.5,158.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCJ3-009","T800","Diesel","10 years / 435,000 mi","Y","N",72.3,45.5,158.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCJ3-009","Model 365","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,158.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCH3-008","C500","Diesel","10 years / 435,000 mi","Y","N",78,45.5,158.3,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCH3-008","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",78,45.5,158.3,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCH3-008","Model 367","Diesel","10 years / 435,000 mi","Y","N",78,45.5,158.3,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCH3-008","W900","Diesel","10 years / 435,000 mi","Y","N",78,45.5,158.3,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCG3-007","Model 367","Diesel","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","PPCR2TRACCG3-007","Model 520","Compressed Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","PPCR2TRACCR6-010","Model 579","Diesel","10 years / 435,000 mi","Y","N",54.1,33.7,111.7,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","PPCR2TRACCR6-010","Model 348","Diesel","10 years / 435,000 mi","Y","N",54.1,33.7,111.7,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV17U","Compression-ignition Heavy HDV - Urban","PDTN2VOCV17U-063","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,233,373,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Vehicle weight reduction"]
[2023,"Daimler Truck North America LLC","PDTN2VOCV17U","Compression-ignition Heavy HDV - Urban","PDTN2VOCV17U-063","Freightliner M2 106/112","Diesel","10 years / 435,000 mi","Y","N",308,233,373,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-01","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PPCR2TRACCX8-016","Model 520","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2023,"PACCAR Inc","PPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PPCR2TRACCX8-016","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PPCR2TRACCX8-016","Model 330","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","PPCR2TRACCX8-016","C500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCA1-001","T270","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,76.3,218.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCA1-001","Model 220","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,76.3,218.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCA1-001","Model 389","Diesel","10 years / 185,000 mi","Y","N",113.5,76.3,218.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023," BYD Auto Industry Company Limited","PBYD2VOCVHRC","Compression-ignition Heavy HDV - Regional","PBYD2VOCVHRC-003","BYD Electric Coach 45 Ft.","Electricity","10 years / 435,000 mi","Y","N",205,0,0,"Application for BYD Electric Coach 35 Ft., BYD Electric Double-decker Coach 35 Ft., BYD Electric Coach 40 Ft., BYD Electric Coach 45 Ft., and BYD Electric Double-decker Coach 45 Ft.","Y",0,1,"Y","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"N","N","N","Y","2023-01-01","Low rolling resistance tires (all)"]
[2023,"PACCAR Inc","PPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCF2-006","W990","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,155.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCF2-006","Model 537","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,155.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCE2-005","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,154.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCE2-005","Model 537","Diesel","10 years / 435,000 mi","Y","N",85.4,56.4,154.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCE2-005","Model 579","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,154.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCE2-005","Model 535","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,154.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCD2-004","Model 367","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Aerodynamic roof fairing"]
[2023,"PACCAR Inc","PPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCD2-004","W900","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (drive)"]
[2023,"PACCAR Inc","PPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","PPCR2TRACCD2-004","Model 389","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCC1-003","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,74.3,215.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCC1-003","T440","Diesel","10 years / 185,000 mi","Y","N",105.5,74.3,215.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCC1-003","Model 337","Diesel","10 years / 185,000 mi","Y","N",105.5,74.3,215.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Tire pressure monitoring system"]
[2023,"PACCAR Inc","PPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCC1-003","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,74.3,215.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCB1-002","T880","Diesel","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (steer)"]
[2023,"PACCAR Inc","PPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCB1-002","T800","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Expiring vehicle speed limiter"]
[2023,"PACCAR Inc","PPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCB1-002","Model 536","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle weight reduction"]
[2023,"PACCAR Inc","PPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCB1-002","Model 537","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Low rolling resistance tires (all)"]
[2023,"PACCAR Inc","PPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","PPCR2TRACCB1-002","T370","Diesel","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2023-01-02","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","Model 337","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","Model 537","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","T680","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","T370","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","T470","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","Model 537","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","T680","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","Model 330","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","T680","Diesel","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Engine shutoff after 5 minutes or less of idling"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","C500","Diesel","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","T480","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","T880","Compressed Natural Gas","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","T440","Diesel","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","Model 365","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","NPCR2VOCVC2R-023","Model 548","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","NPCR2VOCVC2R-023","Model 535","Diesel","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","NPCR2VOCVC2R-023","Model 367","Diesel","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","NPCR2VOCVC3R-024","Model 535","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","NPCR2VOCVC3R-024","Model 537","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","NPCR2VOCVC4R-025","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","NPCR2VOCVC4R-025","Model 548","Diesel","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","NPCR2VOCVC4R-025","W900","Diesel","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","NPCR2VOCVC5R-026","C500","Diesel","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","NPCR2VOCVC5R-026","T380","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","NPCR2VOCVC6R-027","Model 220","Diesel","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","NPCR2VOCVC6R-027","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","NPCR2VOCVC6R-027","T380","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","C500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","Model 536","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","Model 330","Diesel","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","Model 330","Diesel","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","Model 365","Diesel","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","T880","Diesel","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","NPCR2TRACCU7-031","W900","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Automatic engine shutdown system"]
[2022,"PACCAR Inc","NPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","NPCR2TRACCU7-031","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","NPCR2TRACCW7-033","C500","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","NPCR2TRACCW7-033","W900","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","NPCR2TRACCT6-030","Model 337","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,149.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","NPCR2TRACCT6-030","Model 567","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,149.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","NPCR2TRACCV7-032","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",47.9,27.1,114.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","NPCR2TRACCV7-032","Model 579","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",47.9,27.1,114.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2VOCVE6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVE6K-013","Model 520","Electricity","10 years / 435,000 mi","Y","N",308,0,0,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2022-04-25","Low rolling resistance tires (all)"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC300","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NVPT2TRAC300-003","Mack Anthem AN (CHX)","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,79.3,119,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 337","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","T280","Diesel","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 520","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","W990","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","Model 548","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","T280","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 579","Diesel","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","T170","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","Model 536","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","Model 348","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","Model 337","Diesel","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","NPCR2VOCVC1K-015","Model 337","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","NPCR2VOCVC1K-015","T480","Diesel","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","NPCR2VOCVC1K-015","Model 220","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","NPCR2VOCVC2K-016","T880","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","NPCR2VOCVC2K-016","Model 567","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","NPCR2VOCVC2K-016","T470","Diesel","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","NPCR2VOCVC3K-017","W990","Diesel","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","NPCR2VOCVC3K-017","T380","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","NPCR2VOCVC3K-017","Model 536","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","Model 220","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","W900","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","K370","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","Model 520","Diesel","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","T440","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","Model 365","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","Model 536","Diesel","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","Model 535","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","NPCR2VOCVC1R-022","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","NPCR2VOCVC1R-022","Model 548","Diesel","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC08E","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC08E-021","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,95.60000000000001,141.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV03S","Compression-ignition Medium HDV - Regional","NDTN2VOCV03S-058","FCCC MBC/MC/MT45/MT55 Chassis","Diesel","10 years / 185,000 mi","Y","N",234,187,282,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05N","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV05N-062","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,216,311,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05S","Compression-ignition Heavy HDV - Regional","NDTN2VOCV05S-060","Western Star 4700SB/4700SF/47X/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Diesel","10 years / 435,000 mi","Y","N",205,185,258,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV16N","Compression-ignition Medium HDV - Multipurpose","NDTN2VOCV16N-066","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,203,323,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV16S","Compression-ignition Medium HDV - Regional","NDTN2VOCV16S-067","Freightliner SD108/SD114/SD122","Diesel","10 years / 185,000 mi","Y","N",234,187,282,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05U","Compression-ignition Heavy HDV - Urban","NDTN2VOCV05U-052","Freightliner M2 106/112","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,242,347,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05R","Compression-ignition Heavy HDV - Regional","NDTN2VOCV05R-054","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,185,258,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05R","Compression-ignition Heavy HDV - Regional","NDTN2VOCV05R-054","FCCC XBA/XBP/XBR/XBS Chassis","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,185,258,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC09E","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC09E-020","Freightliner SD108/SD114/SD122","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.5,70.5,112.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC10E","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC10E-023","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",72.3,57.7,91.8,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC11E","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC11E-022","Western Star 57X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,75.4,109.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC14E","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC14E-028","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",75.7,62.300000000000004,102.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC29E","Class 8 heavy-haul low-roof day cab tractor","NDTN2TRAC29E-027","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",51.800000000000004,43.4,63.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC31E","Class 8 heavy-haul mid-roof day cab tractor","NDTN2TRAC31E-026","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",54.1,48.300000000000004,62.2,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC33E","Class 8 heavy-haul high-roof day cab tractor","NDTN2TRAC33E-031","Western Star 57X","Diesel","10 years / 435,000 mi","Y","N",54.1,48.6,64.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC34E","Class 8 heavy-haul high-roof sleeper cab tractor","NDTN2TRAC34E-030","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,37.800000000000004,59.1,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Daimler Truck North America LLC","NDTN2TRACHHE","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NDTN2TRACHHE-029","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Diesel","10 years / 435,000 mi","Y","N",59.4,45.800000000000004,61.4,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV04N","Compression-ignition Medium HDV - Multipurpose","NDTN2VOCV04N-056","Western Star 4700SB/4700SF","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,203,323,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV04S","Compression-ignition Medium HDV - Regional","NDTN2VOCV04S-061","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,187,282,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05N","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV05N-062","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Diesel","10 years / 435,000 mi","Y","N",261,216,311,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05S","Compression-ignition Heavy HDV - Regional","NDTN2VOCV05S-060","FCCC S2, S2C, S2G, S2RV","Diesel","10 years / 435,000 mi","Y","N",205,185,258,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05V","Compression-ignition Heavy HDV - Urban","NDTN2VOCV05V-064","FCCC XBA/XBP/XBR/XBS Chassis","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,242,347,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV16N","Compression-ignition Medium HDV - Multipurpose","NDTN2VOCV16N-066","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,203,323,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17N","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV17N-069","Western Star 4700SB/4700SF/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,216,311,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC30E","Class 8 heavy-haul low-roof sleeper cab tractor","NDTN2TRAC30E-033","Western Star 57X","Diesel","10 years / 435,000 mi","Y","N",45.300000000000004,38.9,58.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Engine shutoff after 5 minutes or less of idling"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC07E","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC07E-019","Western Star 57X","Diesel","10 years / 185,000 mi","Y","N",113.2,95.10000000000001,132.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC09E","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC09E-020","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,70.5,112.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (steer)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC13E","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC13E-024","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,73.8,108.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC11E","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC11E-022","Western Star 57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,75.4,109.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC14E","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC14E-028","Western Star 57X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",75.7,62.300000000000004,102.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Automatic engine shutdown system"]
[2022,"PACCAR Inc","NPCR2TRACEE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACEE2-014","Model 579","Electricity","10 years / 435,000 mi","Y","N",85.4,0,0,null,"Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2022-01-01","Vehicle speed limiter"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC12C","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC12C-013","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",78,63.1,97.60000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Refuse Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC34C","Class 8 heavy-haul high-roof sleeper cab tractor","NDTN2TRAC34C-005","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",46.9,37.800000000000004,59.1,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC34C","Class 8 heavy-haul high-roof sleeper cab tractor","NDTN2TRAC34C-005","Western Star 57X","Diesel","10 years / 435,000 mi","Y","N",46.9,37.800000000000004,59.1,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Automatic engine shutdown system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV03U","Compression-ignition Medium HDV - Urban","NDTN2VOCV03U-034","Freightliner M2 106/112","Diesel","10 years / 185,000 mi","Y","N",296,220,354,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17R","Compression-ignition Heavy HDV - Regional","NDTN2VOCV17R-035","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",205,185,258,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17M","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV17M-036","Freightliner M2 106/112","Diesel","10 years / 435,000 mi","Y","N",261,216,311,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"PACCAR Inc","NPCR2TRACED2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACED2-010","Model 220","Electricity","10 years / 435,000 mi","Y","N",85.60000000000001,0,0,null,"Y",0,1,"N","N","Y",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2022-01-01","Vehicle speed limiter"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17V","Compression-ignition Heavy HDV - Urban","NDTN2VOCV17V-068","Western Star 4700SB/4700SF/47X/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,242,347,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC07C-002","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,95.10000000000001,132.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC09C","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC09C-014","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",80.5,70.5,112.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC10C-016","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,57.7,91.8,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (steer)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC12C","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC12C-013","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",78,63.1,97.60000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Refuse Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC12C","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC12C-013","Western Star 57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",78,63.1,97.60000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Refuse Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC13C","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC13C-007","Western Star 4700SB/4700SF/47X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,73.8,108.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC06C","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC06C-001","Western Star 57X","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,88.4,124.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC14C","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC14C-006","Western Star 4700SB/4700SF","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",75.7,62.300000000000004,102.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC31C","Class 8 heavy-haul mid-roof day cab tractor","NDTN2TRAC31C-008","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,48.300000000000004,62.2,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC11C","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC11C-012","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,75.4,109.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV04M","Compression-ignition Medium HDV - Multipurpose","NDTN2VOCV04M-044","Freightliner M2 106/112","Diesel","10 years / 185,000 mi","Y","N",265,203,323,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV04R","Compression-ignition Medium HDV - Regional","NDTN2VOCV04R-047","FCCC XBA/XBP/XBR/XBS Chassis","Diesel","10 years / 185,000 mi","Y","N",234,187,282,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05M","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV05M-049","Freightliner EconicSD","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,216,311,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05M","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV05M-049","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",261,216,311,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC07C-002","Western Star 4700SB/4700SF","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.2,95.10000000000001,132.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC08C","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC08C-015","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,95.60000000000001,141.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Daimler Truck North America LLC","NDTN2TRACHHC","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NDTN2TRACHHC-017","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",59.4,45.800000000000004,61.4,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Engine shutoff after 5 minutes or less of idling"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV16M","Compression-ignition Medium HDV - Multipurpose","NDTN2VOCV16M-055","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,203,323,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC06E","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC06E-018","Freightliner M2 106/112","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,88.4,124.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC06E","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC06E-018","Western Star 4700SB/4700SF/47X","Diesel","10 years / 185,000 mi","Y","N",105.5,88.4,124.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC06E","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC06E-018","Western Star 4900EX/4900FA/4900SA/49X","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,88.4,124.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC800","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NVPT2TRAC800-007-R01","Volvo VNL","Compressed Natural Gas","10 years / 435,000 mi","Y","N",78,68.5,114,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2VOCVH00","Compression-ignition Heavy HDV - Urban","NVPT2VOCVH00-016","Mack LRe","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,0,375,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS, ELECTRIC VEHICLES","Y",0,1,"Y","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2022-06-13","Automatic engine shutdown system"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","T370","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","T680","Diesel","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","W990","Diesel","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","T440","Diesel","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","C500","Diesel","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","W900","Diesel","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","T880","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","T380","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Engine shutoff after 5 minutes or less of idling"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","Model 367","Diesel","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","NPCR2TRACCW7-033","Model 567","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","NPCR2TRACCW7-033","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRACR00","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NVPT2TRACR00-021","Volvo VNL 300","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,79.3,119,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","K370","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","W900","Diesel","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","Model 389","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","Model 365","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","Model 348","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","Model 548","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","T380","Diesel","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV04M","Compression-ignition Medium HDV - Multipurpose","NDTN2VOCV04M-044","Thomas Built Buses C2/EFX/HDX","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",265,203,323,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV04U","Compression-ignition Medium HDV - Urban","NDTN2VOCV04U-048","FCCC MBC/MC/MT45/MT55 Chassis","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,220,354,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05R","Compression-ignition Heavy HDV - Regional","NDTN2VOCV05R-054","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,185,258,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05M","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV05M-049","FCCC S2, S2C, S2G, S2RV","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,216,311,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05U","Compression-ignition Heavy HDV - Urban","NDTN2VOCV05U-052","Freightliner EconicSD","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,242,347,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV16R","Compression-ignition Medium HDV - Regional","NDTN2VOCV16R-041","Western Star 4700SB/4700SF/47X/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,187,282,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17U","Compression-ignition Heavy HDV - Urban","NDTN2VOCV17U-043","Freightliner M2 106/112","Diesel","10 years / 435,000 mi","Y","N",308,242,347,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC100","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NVPT2TRAC100-001","VOLVO VNR 300","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,72,116,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-11-28","Vehicle speed limiter"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2VOCVG00","Compression-ignition Heavy HDV - Regional","NVPT2VOCVG00-015","Mack Anthem AN(AB)","Electricity","10 years / 435,000 mi","Y","N",205,0,257,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 537","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 337","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 535","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","Model 535","Diesel","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","Model 337","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","T680","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","Model 520","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","T270","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","Model 330","Diesel","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","T800","Diesel","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 348","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 548","Diesel","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","T470","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","C500","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","Model 220","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","T880","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","Model 330","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","T440","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","Model 348","Diesel","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","Model 367","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","C500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","T440","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","T800","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","Model 348","Diesel","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","Model 389","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","T880","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","Model 365","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","Model 348","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","NPCR2TRACCT6-030","Model 389","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,149.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","NPCR2TRACCT6-030","T800","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,149.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC08E","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC08E-021","Western Star 4700SB/4700SF/47X","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,95.60000000000001,141.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC08E","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC08E-021","Western Star 57X","Diesel","10 years / 185,000 mi","Y","N",113.5,95.60000000000001,141.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRACV00","Class 8 heavy-haul low-roof day cab tractor","NVPT2TRACV00-025-R01","VOLVO VNL 300","Diesel","10 years / 435,000 mi","Y","N",51.800000000000004,46.7,58.4,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","NPCR2TRACCU7-031","Model 389","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","NPCR2TRACCV7-032","Model 579","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",47.9,27.1,114.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","NPCR2TRACCV7-032","T880","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",47.9,27.1,114.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Engine shutoff after 5 minutes or less of idling"]
[2022,"PACCAR Inc","NPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","NPCR2TRACCV7-032","Model 365","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",47.9,27.1,114.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRACQ00","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NVPT2TRACQ00-020","MACK PINNACLE PI","Diesel","10 years / 435,000 mi","Y","N",80.5,72,116,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2VOCVJ00","Compression-ignition Heavy HDV - Multipurpose","NVPT2VOCVJ00-017","Volvo VHD (AF, AB)","Diesel","10 years / 435,000 mi","Y","N",261,0,322,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"Y","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2022-06-13","Tire pressure monitoring system"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC700","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NVPT2TRAC700-006-R02","Mack Pinnacle PI (CHU)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72.3,66.1,114,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC900","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NVPT2TRAC900-008-R02","Mack Pinnacle PI (CHU)","Diesel","10 years / 435,000 mi","Y","N",75.7,67.6,116,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\".","N",null,null,"N",null,"Please refer document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\".",null,null,"Y","Y","N","Y","2022-01-01","Automatic engine shutdown system"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRACN00","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NVPT2TRACN00-011-R02","Mack Pinnacle PI (CHU)","Diesel","10 years / 435,000 mi","Y","N",52.4,46.7,64,"Heavy Haul Applications.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","Model 579","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","T800","Diesel","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCJ3-009","T440","Diesel","10 years / 435,000 mi","Y","N",72.3,45.5,165.20000000000002,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Automatic engine shutdown system"]
[2022,"Motor Coach Industries","NMCH2VOCVMCH","Coach bus","NMCH2VOCVMCH-003-R02","D4000 ISTV","Compressed Natural Gas","10 years / 435,000 mi","Y","N",210,202,224,"Motor coach, ISTV, Over the road bus, charter bus, commuter bus","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-05-04","Low rolling resistance tires (steer)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC08E","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC08E-021","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,95.60000000000001,141.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC09E","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC09E-020","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",80.5,70.5,112.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 365","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","T470","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","T370","Diesel","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 325","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCA1-001","Model 535","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,75.2,217.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","Model 579","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","T270","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCB1-002","T180","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,74.10000000000001,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 365","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 365","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 535","Diesel","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","Model 330","Diesel","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NPCR2TRACCC1-003","W990","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,73.3,214.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","Model 220","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","Model 520","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCD2-004","T470","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.9,171.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","Model 389","Diesel","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","W900","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCE2-005","Model 537","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,56.4,161.4,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","Model 348","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","NPCR2TRACCR6-028","Model 367","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.7,149.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRACV00","Class 8 heavy-haul low-roof day cab tractor","NVPT2TRACV00-025-R01","VOLVO VNR 300","Diesel","10 years / 435,000 mi","Y","N",51.800000000000004,46.7,58.4,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (steer)"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRACY00","Class 8 heavy-haul mid-roof sleeper cab tractor","NVPT2TRACY00-028-R01","Mack Pinnacle PI (CHU)","Diesel","10 years / 435,000 mi","Y","N",47.9,46.7,58.4,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05N","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV05N-062","Western Star 4700SB/4700SF/47X/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Diesel","10 years / 435,000 mi","Y","N",261,216,311,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05S","Compression-ignition Heavy HDV - Regional","NDTN2VOCV05S-060","Western Star 4700SB/4700SF/47X/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Diesel","10 years / 435,000 mi","Y","N",205,185,258,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17N","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV17N-069","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,216,311,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17V","Compression-ignition Heavy HDV - Urban","NDTN2VOCV17V-068","Western Star 4700SB/4700SF/47X/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Diesel","10 years / 435,000 mi","Y","N",308,242,347,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"International Motors, LLC","NNVX2TRACXLW","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NNVX2TRACXLW-019-R01","LS","Diesel","10 years / 435,000 mi","Y","N",78,62.5,110.5,"Tractor","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","Model 365","Diesel","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","W990","Diesel","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","NPCR2TRACCS6-029","Model 337","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.5,149.1,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","NPCR2TRACCT6-030","Model 537","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,149.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","NPCR2TRACCT6-030","W990","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,33.5,149.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","NPCR2TRACCU7-031","T800","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Engine shutoff after 5 minutes or less of idling"]
[2022,"PACCAR Inc","NPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","NPCR2TRACCU7-031","W990","Diesel","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Engine shutoff after 5 minutes or less of idling"]
[2022,"PACCAR Inc","NPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","NPCR2TRACCU7-031","C500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,27.3,115.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","NPCR2TRACCV7-032","Model 367","Diesel","10 years / 435,000 mi","Y","N",47.9,27.1,114.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","NPCR2TRACCV7-032","Model 389","Compressed Natural Gas","10 years / 435,000 mi","Y","N",47.9,27.1,114.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","NPCR2TRACCW7-033","Model 367","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","NPCR2TRACCW7-033","Model 579","Diesel","10 years / 435,000 mi","Y","N",45.300000000000004,27.1,114.5,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NPCR2TRACCX8-020","Model 536","Diesel","10 years / 435,000 mi","Y","N",52.4,33.7,148.3,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","NPCR2VOCVC1K-015","Model 535","Diesel","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC100","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NVPT2TRAC100-001","VOLVO VNL 300","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,72,116,"Bulk and Regional Haul.","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-11-28","Vehicle weight reduction"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC700","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NVPT2TRAC700-006-R02","Volvo VNR","Diesel","10 years / 435,000 mi","Y","N",72.3,62.7,114,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (steer)"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRAC300","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NVPT2TRAC300-003","Volvo VNL 300","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,79.3,111.10000000000001,"Bulk and Regional Haul","Y",0,1,"Y","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","NPCR2VOCVC1K-015","Model 389","Diesel","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","NPCR2VOCVC1K-015","Model 220","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","NPCR2VOCVC1R-022","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","NPCR2VOCVC1R-022","Model 535","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,154,644,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","NPCR2VOCVC2R-023","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","NPCR2VOCVC2R-023","W990","Diesel","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","NPCR2VOCVC2K-016","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","NPCR2VOCVC2K-016","T270","Diesel","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","NPCR2VOCVC2K-016","T280","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,173,664,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","NPCR2VOCVC3K-017","T680","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","NPCR2VOCVC3K-017","Model 536","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","NPCR2VOCVC3K-017","T370","Diesel","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","NPCR2VOCVC3R-024","Model 579","Diesel","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","NPCR2VOCVC3R-024","T380","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","NPCR2VOCVC3R-024","Model 220","Diesel","10 years / 185,000 mi","Y","N",296,210,634,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2TRACT00","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NVPT2TRACT00-023-R01","Volvo VNL","Diesel","10 years / 435,000 mi","Y","N",78,74.2,114,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"","N",null,null,"N",null,"Please refer to document titled \"CBI_NVPT2_COMMON_IDLE_SHUTDOWN_PARAMETERS.pdf\"",null,null,"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC12E","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC12E-025","Western Star 4700SB/4700SF/47X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",78,63.1,97.60000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Refuse Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC14E","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC14E-028","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Diesel","10 years / 435,000 mi","Y","N",75.7,62.300000000000004,102.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"International Motors, LLC","NNVX2VOCVXBU","Compression-ignition Medium HDV - Urban","NNVX2VOCVXBU-010-R01","International LT","Diesel","10 years / 185,000 mi","Y","N",296,238,381,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"International Motors, LLC","NNVX2VOCVXNU","Compression-ignition Class 7 Vocational Tractor - Urban","NNVX2VOCVXNU-043-R01","international HV","Diesel","10 years / 185,000 mi","Y","N",296,238,381,"Heavy Hauler Tractor, On/Off Highway Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (steer)"]
[2022,"International Motors, LLC","NNVX2TRACXHC","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NNVX2TRACXHC-039-R01","HX","Diesel","10 years / 435,000 mi","Y","N",52.4,43.2,66.1,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"International Motors, LLC","NNVX2TRACXJS","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NNVX2TRACXJS-027-R01","LS","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,72.8,119.8,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC06C","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC06C-001","Western Star 4700SB/4700SF/47X","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,88.4,124.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC07C-002","Western Star 4700SB/4700SF/47X","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.2,95.10000000000001,132.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC08C","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC08C-015","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.5,95.60000000000001,141.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (all)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC10C-016","Western Star 57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,57.7,91.8,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC11C","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC11C-012","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",85.4,75.4,109.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC13C","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","NDTN2TRAC13C-007","Western Star 4700SB/4700SF/47X","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,73.8,108.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC14C","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NDTN2TRAC14C-006","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",75.7,62.300000000000004,102.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2022-01-01","Aerodynamic roof fairing"]
[2022,"Daimler Truck North America LLC","NDTN2TRACHHC","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NDTN2TRACHHC-017","Western Star 57X","Diesel","10 years / 435,000 mi","Y","N",52.4,45.800000000000004,61.4,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC29C","Class 8 heavy-haul low-roof day cab tractor","NDTN2TRAC29C-003","Western Star 57X","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,43.4,63.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC33C","Class 8 heavy-haul high-roof day cab tractor","NDTN2TRAC33C-011","Western Star 57X","Diesel","10 years / 435,000 mi","Y","N",54.1,48.6,64.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC33C","Class 8 heavy-haul high-roof day cab tractor","NDTN2TRAC33C-011","Western Star 4700SB/4700SF","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,48.6,64.8,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC30C","Class 8 heavy-haul low-roof sleeper cab tractor","NDTN2TRAC30C-004","Western Star 4700SB/4700SF","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,38.9,58.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05M","Compression-ignition Heavy HDV - Multipurpose","NDTN2VOCV05M-049","Freightliner M2 106/112","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,216,311,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV05U","Compression-ignition Heavy HDV - Urban","NDTN2VOCV05U-052","Western Star 4700SB/4700SF/47X/4900EX/4900FA/4900SA/4900XD/49X/57X/6900XD","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,242,347,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Gap reducing fairing"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17R","Compression-ignition Heavy HDV - Regional","NDTN2VOCV17R-035","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,185,258,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Vehicle weight reduction"]
[2022,"Daimler Truck North America LLC","NDTN2VOCV17R","Compression-ignition Heavy HDV - Regional","NDTN2VOCV17R-035","Freightliner M2 106/112","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,185,258,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","Model 535","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","NPCR2VOCVC4K-018","Model 330","Diesel","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC06E","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","NDTN2TRAC06E-018","Freightliner SD108/SD114/SD122","Diesel","10 years / 185,000 mi","Y","N",105.5,88.4,124.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC29E","Class 8 heavy-haul low-roof day cab tractor","NDTN2TRAC29E-027","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,43.4,63.7,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2022-01-01","Automatic tire inflation system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC30E","Class 8 heavy-haul low-roof sleeper cab tractor","NDTN2TRAC30E-033","Western Star 57X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,38.9,58.5,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Tire pressure monitoring system"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC32E","Class 8 heavy-haul mid-roof sleeper cab tractor","NDTN2TRAC32E-032","Western Star 4700SB/4700SF","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",47.9,38.9,60.1,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Engine shutoff after 5 minutes or less of idling"]
[2022,"Daimler Truck North America LLC","NDTN2TRAC32E","Class 8 heavy-haul mid-roof sleeper cab tractor","NDTN2TRAC32E-032","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",47.9,38.9,60.1,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Low rolling resistance tires (drive)"]
[2022,"Daimler Truck North America LLC","NDTN2TRACHHE","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","NDTN2TRACHHE-029","Western Star 4900EX/4900FA/4900SA/4900XD/49X","Compressed Natural Gas","10 years / 435,000 mi","Y","N",52.4,45.800000000000004,61.4,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2022-01-01","Adjustable height aerodynamic roof fairing"]
[2022,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","NVPT2VOCVG00","Compression-ignition Heavy HDV - Regional","NVPT2VOCVG00-015","Volvo VHD (AF, AB)","Diesel","10 years / 435,000 mi","Y","N",205,0,257,"REGIONAL DISTRIBUTION, DUMP TRUCKS, REFUSE, DELIVERY, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","Y","2022-01-01","Engine shutoff after 5 minutes or less of idling"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","Model 537","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","T680","Diesel","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","Model 535","Diesel","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","NPCR2TRACCF2-006","T370","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80.5,56.6,161.70000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","T800","Diesel","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Aerodynamic roof fairing"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","Model 520","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCG3-007","T380","Diesel","10 years / 435,000 mi","Y","N",75.7,46.4,177,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","T370","Diesel","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Automatic engine shutdown system"]
[2022,"PACCAR Inc","NPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","NPCR2TRACCH3-008","Model 367","Diesel","10 years / 435,000 mi","Y","N",78,45.5,165,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2022-12-26","Gap reducing fairing"]
[2022,"PACCAR Inc","NPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","NPCR2VOCVC4R-025","T380","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","NPCR2VOCVC4R-025","T370","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,139,549,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","Model 330","Diesel","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2022,"PACCAR Inc","NPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","NPCR2VOCVC5K-019","T370","Diesel","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","NPCR2VOCVC5R-026","T380","Diesel","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (drive)"]
[2022,"PACCAR Inc","NPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","NPCR2VOCVC5R-026","Model 579","Diesel","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Vehicle weight reduction"]
[2022,"PACCAR Inc","NPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","NPCR2VOCVC5R-026","Model 337","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",261,175,524,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","T480","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","T470","Diesel","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Expiring vehicle speed limiter"]
[2022,"PACCAR Inc","NPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","NPCR2VOCVC6K-021","Model 337","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (steer)"]
[2022,"PACCAR Inc","NPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","NPCR2VOCVC6R-027","T800","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Low rolling resistance tires (all)"]
[2022,"PACCAR Inc","NPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","NPCR2VOCVC6R-027","T370","Diesel","10 years / 435,000 mi","Y","N",308,205,520,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage, refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2022-12-26","Tire pressure monitoring system"]
[2021,"International Motors, LLC","MNVX2TRACXEM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MNVX2TRACXEM-023-R01","RH","Diesel","10 years / 185,000 mi","Y","N",113.2,97,149.20000000000002,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic roof fairing"]
[2021,"International Motors, LLC","MNVX2TRACXHW","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","MNVX2TRACXHW-026-R01","LT","Diesel","10 years / 435,000 mi","Y","N",85.4,73.3,120.8,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"International Motors, LLC","MNVX2TRACXLA","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","MNVX2TRACXLA-039-R01","LT","Diesel","10 years / 435,000 mi","Y","N",78,64,113.9,"Tractor This is per Canadian requirementÃƒÂ¢Ã¢â€šÂ¬Ã¢â‚¬â„¢ CO2 Emission Standard (g/ton-mile) = 80.8. Classification for Heavy-Line GCWR 97K - 120K.","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2021-01-01","Gap reducing fairing"]
[2021,"International Motors, LLC","MNVX2TRACXMS","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","MNVX2TRACXMS-040-R01","RH","Diesel","10 years / 435,000 mi","Y","N",75.7,63.1,116.8,"Tractor This is per Canadian requirement CO2 Emission Standard (g/ton-mile) = 75.7. Classification for Heavy GCWR < 97K.","Y",0,1,"N","Y","N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System","N",null,null,"N",null,"Information for the Automatic Engine Stop Start  feature is on file in the EPA EV/CIS System",null,null,"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"International Motors, LLC","MNVX2TRACXGW","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","MNVX2TRACXGW-025-R01","RH","Diesel","10 years / 435,000 mi","Y","N",80.5,68.5,115.5,"Tractor","Y",0,1,"N","Y","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2TRACS00","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","MVPT2TRACS00-011","Volvo VNR","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72.3,67.9,91.10000000000001,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Gap reducing fairing"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2TRACQ00","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","MVPT2TRACQ00-010","MACK PINNACLE PI","Diesel","10 years / 435,000 mi","Y","N",80.5,72,99.2,"Bulk and Regional Haul.","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2TRACZ00","Class 8 heavy-haul high-roof sleeper cab tractor","MVPT2TRACZ00-028","Mack Pinnacle PI (CHU)","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,47.9,58.4,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Gap reducing fairing"]
[2021,"Isuzu Motors Limited","MSZX2VOCVLD2","Compression-ignition Light HDV - Urban","MSZX2VOCVLD2-004","HINO S41","Diesel","15 years / 150,000 mi","Y","N",424,337,344,"BOX DELIVERY, LANDSCAPE UTILITY, REFER, FURNITURE, TOW, FLATBED, MULTI-STOP","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-07-02","Vehicle weight reduction"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2TRACX00","Class 8 heavy-haul low-roof sleeper cab tractor","MVPT2TRACX00-027","Mack Pinnacle PI (CHU)","Diesel","10 years / 435,000 mi","Y","N",45.300000000000004,47.9,58.4,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"Kovatch Mobile Equipment Corporation","MKME2VOCV001","Emergency vehicle","MKME2VOCV001-001","Rescue","Diesel","10 years / 435,000 mi","N","N",324,310,324,"All vehicles in this family are emergency vehicles used in the firefighting industry.","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"N","N","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"Daimler Truck North America LLC","MDTN2VOCV17R","Compression-ignition Heavy HDV - Regional","MDTN2VOCV17R-024","Freightliner SD108/SD114/SD122","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,172,261,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Automatic tire inflation system"]
[2021,"Daimler Truck North America LLC","MDTN2VOCV16M","Compression-ignition Medium HDV - Multipurpose","MDTN2VOCV16M-029","Freightliner Cascadia 113/125/116/126","Diesel","10 years / 185,000 mi","Y","N",265,186,333,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","MDTN2TRAC10C-019","Western Star 4900EX/4900FA/4900SA","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72.3,60.5,92.10000000000001,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2021-01-01","Automatic tire inflation system"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","MDTN2TRAC10C-019","Western Star 4700SB/4700SF","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,60.5,92.10000000000001,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"PACCAR Inc","MPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","MPCR2VOCVC6R-026","Model 220","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,197,553,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","MPCR2VOCVC6R-026","Model 389","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,197,553,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2VOCVC6R","Class 8 Vocational Tractor - Urban","MPCR2VOCVC6R-026","Model 537","Compressed Natural Gas","10 years / 435,000 mi","Y","N",308,197,553,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","MPCR2VOCVC5R-025","W990","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,166,569,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2VOCVC5R","Class 8 Vocational Tractor - Multipurpose","MPCR2VOCVC5R-025","T440","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,166,569,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","MPCR2VOCVC3R-023","Model 220","Diesel","10 years / 185,000 mi","Y","N",296,208,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","MPCR2VOCVC3R-023","T800","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,208,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","MPCR2VOCVC3R-023","T480","Diesel","10 years / 185,000 mi","Y","N",296,208,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2VOCVC3R","Compression-ignition Class 7 Vocational Tractor - Urban","MPCR2VOCVC3R-023","Model 325","Compressed Natural Gas","10 years / 185,000 mi","Y","N",296,208,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2VOCVC4R","Class 8 Vocational Tractor - Regional","MPCR2VOCVC4R-024","Model 537","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,129,552,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","MPCR2VOCVC1R-021","W990","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,154,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","MPCR2VOCVC1R-021","Model 537","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,154,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2VOCVC1R","Compression-ignition Class 7 Vocational Tractor - Regional","MPCR2VOCVC1R-021","Model 337","Diesel","10 years / 185,000 mi","Y","N",234,154,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","MPCR2VOCVC2R-022","W900","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",265,171,562,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2VOCVC2R","Compression-ignition Class 7 Vocational Tractor - Multipurpose","MPCR2VOCVC2R-022","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,171,562,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","MPCR2VOCVC4K-016","T470","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",205,129,552,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","MPCR2VOCVC4K-016","Model 520","Diesel","10 years / 435,000 mi","Y","N",205,129,552,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2VOCVC4K","Compression-ignition Heavy HDV - Regional","MPCR2VOCVC4K-016","Model 330","Compressed Natural Gas","10 years / 435,000 mi","Y","N",205,129,552,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","MPCR2VOCVC5K-017","Model 389","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,166,569,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2VOCVC5K","Compression-ignition Heavy HDV - Multipurpose","MPCR2VOCVC5K-017","Model 367","Compressed Natural Gas","10 years / 435,000 mi","Y","N",261,166,569,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","MPCR2VOCVC6K-020","C500","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,197,553,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","MPCR2VOCVC6K-020","Model 367","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,197,553,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2VOCVC6K","Compression-ignition Heavy HDV - Urban","MPCR2VOCVC6K-020","Model 548","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",308,197,553,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","MPCR2VOCVC2K-014","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,171,562,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","MPCR2VOCVC2K-014","W900","Diesel","10 years / 185,000 mi","Y","N",265,171,562,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2VOCVC2K","Compression-ignition Medium HDV - Multipurpose","MPCR2VOCVC2K-014","Model 537","Compressed Natural Gas","10 years / 185,000 mi","Y","N",265,171,562,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","MPCR2VOCVC3K-015","K270","Diesel","10 years / 185,000 mi","Y","N",296,208,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","MPCR2VOCVC3K-015","Model 579","Diesel","10 years / 185,000 mi","Y","N",296,208,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2VOCVC3K","Compression-ignition Medium HDV - Urban","MPCR2VOCVC3K-015","Model 537","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",296,208,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","MPCR2VOCVC1K-018","Model 325","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,154,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","MPCR2VOCVC1K-018","Model 548","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",234,154,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2VOCVC1K","Compression-ignition Medium HDV - Regional","MPCR2VOCVC1K-018","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,154,550,"Construction, refuse, pickup & delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler, beverage,  refuse, port/drayage, chip hauler","Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCJ3-013","Model 367","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,209.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCJ3-013","Model 579","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72.3,45.5,209.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Aerodynamic roof fairing"]
[2021,"PACCAR Inc","MPCR2TRACCJ3","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCJ3-013","C500","Diesel","10 years / 435,000 mi","Y","N",72.3,45.5,209.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCH3-019","W900","Diesel","10 years / 435,000 mi","Y","N",78,45.4,186.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Engine shutoff after 5 minutes or less of idling"]
[2021,"PACCAR Inc","MPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCH3-019","T470","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",78,45.4,186.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2TRACCH3","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCH3-019","T380","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",78,45.4,186.4,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCG3-012","T800","Diesel","10 years / 435,000 mi","Y","N",75.7,46.6,213.8,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"PACCAR Inc","MPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCG3-012","T440","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.6,213.8,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCG3","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","MPCR2TRACCG3-012","W900","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",75.7,46.6,213.8,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"PACCAR Inc","MPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCF2-011","Model 348","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,55.7,183.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCF2-011","T680","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,55.7,183.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCF2","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCF2-011","Model 579","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,55.7,183.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","MPCR2TRACCU7-029","W900","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",46.9,27,148.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","MPCR2TRACCU7-029","W900","Diesel","10 years / 435,000 mi","Y","N",46.9,27,148.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Engine shutoff after 5 minutes or less of idling"]
[2021,"PACCAR Inc","MPCR2TRACCU7","Class 8 heavy-haul high-roof sleeper cab tractor","MPCR2TRACCU7-029","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",46.9,27,148.6,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","MPCR2TRACCT6-033","Model 337","Diesel","10 years / 435,000 mi","Y","N",51.800000000000004,31.8,140.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","MPCR2TRACCT6-033","Model 367","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,31.8,140.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2TRACCT6","Class 8 heavy-haul low-roof day cab tractor","MPCR2TRACCT6-033","W900","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,31.8,140.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"PACCAR Inc","MPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","MPCR2TRACCX8-028","Model 330","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",52.4,32.2,398.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2TRACCX8","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","MPCR2TRACCX8-028","Model 389","Diesel","10 years / 435,000 mi","Y","N",52.4,32.2,398.6,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","MPCR2TRACCW7-027","W900","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,26.6,147.3,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","MPCR2TRACCW7-027","Model 567","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,26.6,147.3,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"PACCAR Inc","MPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","MPCR2TRACCS6-032","Model 220","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",54.1,31.8,139.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","MPCR2TRACCS6-032","Model 337","Diesel","10 years / 435,000 mi","Y","N",54.1,31.8,139.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic roof fairing"]
[2021,"PACCAR Inc","MPCR2TRACCS6","Class 8 heavy-haul mid-roof day cab tractor","MPCR2TRACCS6-032","Model 330","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,31.8,139.9,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","MPCR2TRACCR6-031","Model 548","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,33.1,141.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Gap reducing fairing"]
[2021,"PACCAR Inc","MPCR2TRACCR6","Class 8 heavy-haul high-roof day cab tractor","MPCR2TRACCR6-031","Model 567","Diesel","10 years / 435,000 mi","Y","N",54.1,33.1,141.5,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"Daimler Truck North America LLC","MDTN2VOCV04U","Compression-ignition Medium HDV - Urban","MDTN2VOCV04U-003","FCCC MBC/MC/MT45/MT55 Chassis","Diesel","10 years / 185,000 mi","Y","N",296,198,371,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Gap reducing fairing"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC14C","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","MDTN2TRAC14C-004","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",75.7,60.800000000000004,103.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"Daimler Truck North America LLC","MDTN2VOCV04M","Compression-ignition Medium HDV - Multipurpose","MDTN2VOCV04M-001","Freightliner SD108/SD114/SD122","Diesel","10 years / 185,000 mi","Y","N",265,186,333,"City Transit Bus Pickup and Delivery Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Automatic tire inflation system"]
[2021,"PACCAR Inc","MPCR2TRACCW7","Class 8 heavy-haul low-roof sleeper cab tractor","MPCR2TRACCW7-027","Model 579","Compressed Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,26.6,147.3,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2TRACCV7","Class 8 heavy-haul mid-roof sleeper cab tractor","MPCR2TRACCV7-030","W900","Diesel","10 years / 435,000 mi","Y","N",47.9,26.6,147.1,null,"Y",0,1,"N","Y","Y",null,"The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.",null,null,"Y","Y","N","Y","2021-01-01","Aerodynamic roof fairing"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2VOCVM00","Compression-ignition Heavy HDV - Multipurpose","MVPT2VOCVM00-022","Volvo VAH (AF,AB)","Diesel","10 years / 435,000 mi","Y","N",261,233,322,"MULTIPURPOSE DISTRIBITION, UTILITY TRUCKS","Y",0,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2TRAC700","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","MVPT2TRAC700-005","Volvo VNL","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72.3,67.9,91.10000000000001,"Bulk and Regional Haul","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2TRACN00","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","MVPT2TRACN00-009","Mack Pinnacle PI (CHU)","Diesel","10 years / 435,000 mi","Y","N",52.4,47.9,58.4,"Heavy Haul Applications.","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","MVPT2TRACQ00","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","MVPT2TRACQ00-010","VOLVO VNL 300","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,72,99.2,"Bulk and Regional Haul.","Y",0,1,"N","N","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"PACCAR Inc","MPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCE2-010","Model 365","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,55.6,183.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic roof fairing"]
[2021,"PACCAR Inc","MPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCE2-010","W990","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,55.6,183.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCE2-010","Model 337","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,55.6,183.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2TRACCE2","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCE2-010","Model 537","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",85.4,55.6,183.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCD2-009","Model 535","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.5,206.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCD2-009","T480","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.60000000000001,57.5,206.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCD2","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","MPCR2TRACCD2-009","T680","Diesel","10 years / 435,000 mi","Y","N",85.60000000000001,57.5,206.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Expiring vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCC1-008","T440","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,71.7,210.8,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (drive)"]
[2021,"PACCAR Inc","MPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCC1-008","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",105.5,71.7,210.8,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"PACCAR Inc","MPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCC1-008","Model 536","Compressed Natural Gas","10 years / 185,000 mi","Y","N",105.5,71.7,210.8,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"PACCAR Inc","MPCR2TRACCC1","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCC1-008","Model 579","Diesel","10 years / 185,000 mi","Y","N",105.5,71.7,210.8,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"PACCAR Inc","MPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCB1-007","T680","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",113.2,71.3,210.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCB1-007","T800","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,71.3,210.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCB1-007","Model 220","Diesel","10 years / 185,000 mi","Y","N",113.2,71.3,210.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle speed limiter"]
[2021,"PACCAR Inc","MPCR2TRACCB1","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCB1-007","Model 536","Diesel","10 years / 185,000 mi","Y","N",113.2,71.3,210.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic roof fairing"]
[2021,"PACCAR Inc","MPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCA1-006","Model 579","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,74,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"PACCAR Inc","MPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCA1-006","W900","Diesel","10 years / 185,000 mi","Y","N",113.5,74,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Gap reducing fairing"]
[2021,"PACCAR Inc","MPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCA1-006","Model 548","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.5,74,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"PACCAR Inc","MPCR2TRACCA1","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MPCR2TRACCA1-006","W990","Diesel","10 years / 185,000 mi","Y","N",113.5,74,215.20000000000002,null,"Y",0,1,"N","Y","Y",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"Daimler Truck North America LLC","MDTN2VOCV17U","Compression-ignition Heavy HDV - Urban","MDTN2VOCV17U-025","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",308,226,347,"Short Haul Service/Recreation Service/ Rescue and Emergency Maintenance Service Construction Service Airport Service Farm Service Mining Service/Refuse Service Fire Service Utility Repair/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Line Haul/Long Haul Service Mobile Lab Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Vehicle weight reduction"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC34C","Class 8 heavy-haul high-roof sleeper cab tractor","MDTN2TRAC34C-011","Western Star 5700XE","Diesel","10 years / 435,000 mi","Y","N",46.9,37.7,55.2,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC33C","Class 8 heavy-haul high-roof day cab tractor","MDTN2TRAC33C-010","Western Star 4900EX/4900FA/4900SA","Diesel","10 years / 435,000 mi","Y","N",54.1,45.1,59.6,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2021-01-01","Gap reducing fairing"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC32C","Class 8 heavy-haul mid-roof sleeper cab tractor","MDTN2TRAC32C-009","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",47.9,38.9,58.800000000000004,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC31C","Class 8 heavy-haul mid-roof day cab tractor","MDTN2TRAC31C-015","Western Star 5700XE","Compressed Natural Gas","10 years / 435,000 mi","Y","N",54.1,44.800000000000004,57.800000000000004,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC30C","Class 8 heavy-haul low-roof sleeper cab tractor","MDTN2TRAC30C-014","Freightliner Cascadia 116/126","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",45.300000000000004,41,57.2,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2021-01-01","Vehicle weight reduction"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC29C","Class 8 heavy-haul low-roof day cab tractor","MDTN2TRAC29C-008","Freightliner SD108/SD114/SD122","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",51.800000000000004,43.4,63,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","Y","Y","2021-01-01","Low rolling resistance tires (all)"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC11C","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","MDTN2TRAC11C-007","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 435,000 mi","Y","N",85.4,75,105,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Low rolling resistance tires (steer)"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC09C","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","MDTN2TRAC09C-018","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80.5,68.2,112.10000000000001,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Tire pressure monitoring system"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC08C","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MDTN2TRAC08C-017","Freightliner Cascadia 116/126","Diesel","10 years / 185,000 mi","Y","N",113.5,96.9,143,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Aerodynamic side skirt and/or fuel tank fairing"]
[2021,"Daimler Truck North America LLC","MDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","MDTN2TRAC07C-016","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 185,000 mi","Y","N",113.2,96.3,132.6,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,null,"N",null,null,"N",{"$nulls":4},"Y","Y","N","Y","2021-01-01","Automatic tire inflation system"]
[2021,"Daimler Truck North America LLC","MDTN2TRACHHC","Class 8 heavy-haul tractor at or above 120,000 pounds GCWR","MDTN2TRACHHC-012","Western Star 4700SB/4700SF","Diesel","10 years / 435,000 mi","Y","N",75.7,60.800000000000004,103.9,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"N","N","N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1","N",null,null,"N",null,"DETROIT/DTNA Proprietary System Refer to File Name AECD_DTN_EXTIDLE_1",null,null,"Y","Y","Y","Y","2021-01-01","Vehicle weight reduction"]
[2021,"New Flyer of America Inc.","MNFA2VOCV004","Transit and other bus","MNFA2VOCV004-004-R01","New Flyer Xcelsior XT35","Hydrogen","10 years / 435,000 mi","Y","N",300,0,0,"Battery-Electric, Hydrogen-Electric and Trackless Electric-Trolley Powered Heavy Duty Urban Transit Buses","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","Y","N","N","2020-11-01","Vehicle weight reduction"]
[2021,"GILLIG LLC","MGLG2VOCVEV1","Transit and other bus","MGLG2VOCVEV1-001","LOW FLOOR ELECTRIC","Electricity","10 years / 435,000 mi","Y","N",300,0,0,"Transit bus","Y",0,1,"N","N","N",null,null,"N",null,null,"Y","Electric Vehicle",{"$nulls":3},"Y","N","N","Y","2021-01-01","Tire pressure monitoring system"]
[2020,"International Motors, LLC","LNVX2TRACXXL","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","LNVX2TRACXXL-008","International LT","Diesel","10 years / 435,000 mi","Y","N",73,58,86,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KNVX2TRACXXM","Y","Y",null,"Y","2019-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2020,"International Motors, LLC","LNVX2TRACXXF","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LNVX2TRACXXF-003","International MV","Diesel","10 years / 185,000 mi","Y","N",120,95,138,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2019-01-02","Vehicle speed limiter"]
[2020,"PACCAR Inc","LPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LPCR2TRAC7DH-002","Model 579","Compressed Natural Gas","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2019-01-02","Aerodynamic roof fairing"]
[2020,"PACCAR Inc","LPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LPCR2TRAC7DH-002","W990","Diesel","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2019-01-02","Aerodynamic roof fairing"]
[2020,"PACCAR Inc","LPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LPCR2TRAC7DH-002","T440","Diesel","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2019-01-02","Low rolling resistance tires"]
[2020,"PACCAR Inc","LPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LPCR2TRAC7DL-003","Model 384","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","LPCR2TRAC7DH","Y","Y",null,"Y","2019-01-02","Gap reducing fairing"]
[2020,"PACCAR Inc","LPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LPCR2TRAC7DM-004","Model 389","Diesel","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","LPCR2TRAC7DH","Y","Y",null,"Y","2019-01-02","Vehicle weight reduction"]
[2020,"PACCAR Inc","LPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LPCR2TRAC7DM-004","T470","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","LPCR2TRAC7DH","Y","Y",null,"Y","2019-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","LPCR2TRAC8DH-007","T660","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2019-01-02","Vehicle weight reduction"]
[2020,"PACCAR Inc","LPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","LPCR2TRAC8DH-007","963","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2019-01-02","Low rolling resistance tires"]
[2020,"PACCAR Inc","LPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","LPCR2TRAC8DL-008","Model 337","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","LPCR2TRAC8DH","Y","Y",null,"Y","2019-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","LPCR2TRAC8DL-008","T680","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","LPCR2TRAC8DH","Y","Y",null,"Y","2019-01-02","Aerodynamic roof fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","LPCR2TRAC8DM-009","T470","Diesel","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","LPCR2TRAC8DH","Y","Y",null,"Y","2019-01-02","Aerodynamic roof fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","LPCR2TRAC8DM-009","T370","Compressed Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","LPCR2TRAC8DH","Y","Y",null,"Y","2019-01-02","Aerodynamic roof fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","LPCR2TRAC8SH-010","T470","Diesel","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2019-01-02","Aerodynamic roof fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","LPCR2TRAC8SH-010","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2019-01-02","Automatic engine shutdown system"]
[2020,"PACCAR Inc","LPCR2TRAC8SL","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","LPCR2TRAC8SL-011","C500","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",66,47,79,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","LPCR2TRAC8SH","Y","Y",null,"Y","2019-01-02","Vehicle weight reduction"]
[2020,"PACCAR Inc","LPCR2TRAC8SL","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","LPCR2TRAC8SL-011","T660","Diesel","10 years / 435,000 mi","Y","N",66,47,79,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","LPCR2TRAC8SH","Y","Y",null,"Y","2019-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","LPCR2TRAC8SM-012","W900","Diesel","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","LPCR2TRAC8SH","Y","Y",null,"Y","2019-01-02","Gap reducing fairing"]
[2020,"PACCAR Inc","LPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","LPCR2TRAC8SM-012","T440","Compressed Natural Gas","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","LPCR2TRAC8SH","Y","Y",null,"Y","2019-01-02","Low rolling resistance tires"]
[2020,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","LVPT2VOCVD00","Class 8 vocational tractors","LVPT2VOCVD00-007","Mack Granite (AF, AB)","Diesel","10 years / 435,000 mi","Y","N",222,203,238,"dump trailers, refuse and recycling, logging, dry and liquid bulk, heavy transport, autohauler, construction equipment/material haulage, urban distribution","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2019-01-02","Low rolling resistance tires"]
[2020,"International Motors, LLC","LNVX2TRACXXE","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LNVX2TRACXXE-002","International ProStar","Diesel","10 years / 185,000 mi","Y","N",115,108,123,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXF","Y","Y",null,"Y","2019-01-02","Vehicle speed limiter"]
[2020,"PACCAR Inc","LPCR2VOCV8TK","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","LPCR2VOCV8TK-013","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,203,237,"Construction, refuse, pickup and delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2019-01-02","Low rolling resistance tires"]
[2020,"PACCAR Inc","LPCR2VOCV8TR","Class 8 vocational tractors","LPCR2VOCV8TR-014","T440","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,203,237,"Construction, heavy haul, pickup and delivery, beverage, utility, logger, mining, oil field, refuse, crane, agriculture, port/drayage, chip hauler","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2019-01-02","Low rolling resistance tires"]
[2020,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","LVPT2TRAC100","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","LVPT2TRAC100-004","VOLVO VNR 300","Diesel","10 years / 435,000 mi","Y","N",80,72,88,"Bulk and Regional Haul","N",null,1,"N","N","N","N",null,"N",null,null,"N",null,null,"Y","LVPT2TRAC900","Y","Y",null,"Y","2019-01-02","Low rolling resistance tires"]
[2020,"Daimler Truck North America LLC","LDTN2TRAC09C","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","LDTN2TRAC09C-004","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80,73,96,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2019-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2020,"International Motors, LLC","LNVX2TRACIXJ","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","LNVX2TRACIXJ-017","International LT","Diesel","10 years / 435,000 mi","Y","N",89,73,103,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"N",null,"Y","Y","N","Y","2019-01-02","Vehicle speed limiter"]
[2020,"International Motors, LLC","LNVX2TRACIXJ","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","LNVX2TRACIXJ-017","International DuraStar","Diesel","10 years / 435,000 mi","Y","N",89,73,103,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"N",null,"Y","Y","N","Y","2019-01-02","Low rolling resistance tires"]
[2020,"International Motors, LLC","LNVX2TRACIXE","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LNVX2TRACIXE-013","International RH","Diesel","10 years / 185,000 mi","Y","N",115,108,123,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXF","Y","Y","N","Y","2019-01-02","Vehicle speed limiter"]
[2020,"Daimler Truck North America LLC","LDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","LDTN2VOCV05C-012","Freightliner Cascadia 116/126","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2019-01-02","Low rolling resistance tires"]
[2020,"Daimler Truck North America LLC","LDTN2TRAC13C","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","LDTN2TRAC13C-008","Western Star 5700XE","Compressed Natural Gas","10 years / 435,000 mi","Y","N",89,79,115,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2019-01-02","Vehicle weight reduction"]
[2020,"Daimler Truck North America LLC","LDTN2TRAC11C","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","LDTN2TRAC11C-006","Western Star 4900EX/4900FA/4900SA","Diesel","10 years / 435,000 mi","Y","N",86,79,103,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2019-01-02","Low rolling resistance tires"]
[2020,"Daimler Truck North America LLC","LDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LDTN2TRAC07C-002","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",115,105,134,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2019-01-02","Low rolling resistance tires"]
[2020,"Daimler Truck North America LLC","LDTN2TRAC06C","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","LDTN2TRAC06C-001","Western Star 4700SB/4700SF","Diesel","10 years / 185,000 mi","Y","N",104,96,124,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2019-01-02","Aerodynamic roof fairing"]
[2020,"International Motors, LLC","LNVX2TRACXXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","LNVX2TRACXXK-007","International ProStar","Diesel","10 years / 435,000 mi","Y","N",66,52,78,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXM","Y","Y",null,"Y","2019-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2020,"International Motors, LLC","LNVX2TRACXXL","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","LNVX2TRACXXL-008","International LT","Diesel","10 years / 435,000 mi","Y","N",73,58,86,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KNVX2TRACXXM","Y","Y",null,"Y","2019-01-02","Low rolling resistance tires"]
[2020,"International Motors, LLC","LNVX2TRACXXG","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","LNVX2TRACXXG-004","International LS","Diesel","10 years / 435,000 mi","Y","N",80,68,86,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KNVX2TRACXXJ","Y","Y",null,"Y","2019-01-02","Gap reducing fairing"]
[2019,"International Motors, LLC","KNVX2VOCVXXB","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","KNVX2VOCVXXB-001","IC School Bus (CE and RE)","Diesel","10 years / 185,000 mi","Y","N",225,211,238,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2018-01-02","Low rolling resistance tires"]
[2019,"Eldorado National-California Inc.","KEDR2VOCV002","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","KEDR2VOCV002-002","XHF CNG","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2018-12-03","Low rolling resistance tires"]
[2019,"International Motors, LLC","KNVX2TRACIXG","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","KNVX2TRACIXG-020","International LS","Diesel","10 years / 435,000 mi","Y","N",80,68,85,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXJ","Y","Y","N","Y","2018-01-02","Vehicle speed limiter"]
[2019,"International Motors, LLC","KNVX2TRACIXF","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KNVX2TRACIXF-019","International DuraStar","Diesel","10 years / 185,000 mi","Y","N",120,105,132,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"N",null,"Y","Y","N","Y","2018-01-02","Low rolling resistance tires"]
[2019,"International Motors, LLC","KNVX2VOCVXXB","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","KNVX2VOCVXXB-001","International CV","Diesel","10 years / 185,000 mi","Y","N",225,211,238,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2018-01-02","Low rolling resistance tires"]
[2019,"International Motors, LLC","KNVX2TRACIXM","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","KNVX2TRACIXM-024","International ProStar","Diesel","10 years / 435,000 mi","Y","N",72,54,95,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"N",null,"Y","Y","N","Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"International Motors, LLC","KNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","KNVX2TRACIXK-022","International LS","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"International Motors, LLC","KNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","KNVX2TRACIXK-022","International LoneStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2018-01-02","Gap reducing fairing"]
[2019,"Daimler Truck North America LLC","KDTN2TRAC12C","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","KDTN2TRAC12C-013","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 435,000 mi","Y","N",73,72,98,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Refuse Service Heavy Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC14C","Y","Y",null,"Y","2018-01-02","Low rolling resistance tires"]
[2019,"Daimler Truck North America LLC","KDTN2TRAC09C","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","KDTN2TRAC09C-010","Western Star 4900EX/4900FA/4900SA","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,73,96,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2018-01-02","Low rolling resistance tires"]
[2019,"Daimler Truck North America LLC","KDTN2VOCV16C","Class 7 vocational tractors","KDTN2VOCV16C-005","Western Star 4900EX/4900FA/4900SA","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2018-01-02","Low rolling resistance tires"]
[2019,"International Motors, LLC","KNVX2TRACIXJ","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","KNVX2TRACIXJ-021","International ProStar","Diesel","10 years / 435,000 mi","Y","N",89,73,103,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","automatic tire inflation system","see 12/1/16 email from Ron Schaefer. Automatic tire inflation system credit allowed per 1037.150(y)","N",null,null,"N",null,"Y","Y","N","Y","2018-01-02","Low rolling resistance tires"]
[2019,"International Motors, LLC","KNVX2TRACXXJ","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","KNVX2TRACXXJ-013","International MV","Diesel","10 years / 435,000 mi","Y","N",89,73,103,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Gap reducing fairing"]
[2019,"PACCAR Inc","KPCR2VOCV8TR","Class 8 vocational tractors","KPCR2VOCV8TR-013","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,203,237,"Construction, heavy haul, pickup and delivery, beverage, utility, logger, mining, oil field, refuse, crane, agriculture, port/drayage, chip hauler","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2018-01-02","Low rolling resistance tires"]
[2019,"PACCAR Inc","KPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","KPCR2TRAC8SM-008","K500","Diesel","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","KPCR2TRAC8SH","Y","Y",null,"Y","2018-01-02","Vehicle speed limiter"]
[2019,"PACCAR Inc","KPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","KPCR2TRAC8SM-008","T440","Compressed Natural Gas","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","KPCR2TRAC8SH","Y","Y",null,"Y","2018-01-02","Automatic engine shutdown system"]
[2019,"PACCAR Inc","KPCR2TRAC8SL","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","KPCR2TRAC8SL-007","Model 384","Compressed Natural Gas","10 years / 435,000 mi","Y","N",66,47,79,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","KPCR2TRAC8SH","Y","Y",null,"Y","2018-01-02","Aerodynamic roof fairing"]
[2019,"PACCAR Inc","KPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","KPCR2TRAC8SH-014","K500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2018-01-02","Vehicle weight reduction"]
[2019,"PACCAR Inc","KPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","KPCR2TRAC8SH-014","T800","Diesel","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2018-01-02","Vehicle weight reduction"]
[2019,"PACCAR Inc","KPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","KPCR2TRAC8DM-006","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KPCR2TRAC8DH","Y","Y",null,"Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"PACCAR Inc","KPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","KPCR2TRAC8DM-006","T660","Compressed Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KPCR2TRAC8DH","Y","Y",null,"Y","2018-01-02","Vehicle speed limiter"]
[2019,"PACCAR Inc","KPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","KPCR2TRAC8DM-006","T680","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KPCR2TRAC8DH","Y","Y",null,"Y","2018-01-02","Vehicle speed limiter"]
[2019,"PACCAR Inc","KPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","KPCR2TRAC8DL-005","Model 382","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KPCR2TRAC8DH","Y","Y",null,"Y","2018-01-02","Vehicle weight reduction"]
[2019,"PACCAR Inc","KPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","KPCR2TRAC8DH-004","Model 367","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"PACCAR Inc","KPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","KPCR2TRAC8DH-004","Model 382","Compressed Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"PACCAR Inc","KPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","KPCR2TRAC8DH-004","T370","Compressed Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Gap reducing fairing"]
[2019,"PACCAR Inc","KPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KPCR2TRAC7DM-003","T800","Compressed Natural Gas","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KPCR2TRAC7DH","Y","Y",null,"Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"PACCAR Inc","KPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KPCR2TRAC7DM-003","Model 579","Diesel","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KPCR2TRAC7DH","Y","Y",null,"Y","2018-01-02","Vehicle weight reduction"]
[2019,"PACCAR Inc","KPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KPCR2TRAC7DL-002","T800","Compressed Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","KPCR2TRAC7DH","Y","Y",null,"Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"PACCAR Inc","KPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KPCR2TRAC7DH-001","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2019,"PACCAR Inc","KPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KPCR2TRAC7DH-001","Model 337","Diesel","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Vehicle weight reduction"]
[2019,"International Motors, LLC","KNVX2VOCVIXB","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","KNVX2VOCVIXB-004","International WorkStar","Diesel","10 years / 185,000 mi","Y","N",225,211,238,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",{"$nulls":8},"2018-01-02","Innovative technologies"]
[2019,"International Motors, LLC","KNVX2VOCVIXC","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","KNVX2VOCVIXC-005","International Stripped Chassis (FBTC)","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Dry Van, Pick-up Delivery, Utility/Service, Beverage, Dump, Plow/Spreader, Refuse, Mixer, Bus, Wrecker, Heavy Haul, Forestry, Oil Field, Construction","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology ?????? Clutched Air Compressor\"","N",{"$nulls":8},"2018-01-02","Innovative technologies"]
[2019,"International Motors, LLC","KNVX2TRACIXJ","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","KNVX2TRACIXJ-021","International LoneStar","Diesel","10 years / 435,000 mi","Y","N",89,73,103,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"N",null,"Y","Y","N","Y","2018-01-02","Low rolling resistance tires"]
[2019,"International Motors, LLC","KNVX2TRACIXE","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KNVX2TRACIXE-018","International ProStar","Diesel","10 years / 185,000 mi","Y","N",115,108,123,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXF","Y","Y","N","Y","2018-01-02","Gap reducing fairing"]
[2019,"Daimler Truck North America LLC","KDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","KDTN2TRAC10C-011","Western Star 5700XE","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",66,64,89,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Aerodynamic roof fairing"]
[2019,"Daimler Truck North America LLC","KDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","KDTN2TRAC10C-011","Freightliner SD108/SD114/SD122","Diesel","10 years / 435,000 mi","Y","N",66,64,89,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2018-01-02","Vehicle weight reduction"]
[2019,"Daimler Truck North America LLC","KDTN2TRAC06C","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","KDTN2TRAC06C-007","Freightliner SD108/SD114/SD122","Diesel","10 years / 185,000 mi","Y","N",104,96,124,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2018-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"International Motors, LLC","JNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACIXK-022","International 9900","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2017-01-02","Low rolling resistance tires"]
[2018,"International Motors, LLC","JNVX2TRACXXE","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JNVX2TRACXXE-006","International LT","Diesel","10 years / 185,000 mi","Y","N",115,108,123,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXF","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"International Motors, LLC","JNVX2VOCVIXC","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","JNVX2VOCVIXC-010","International HX Series","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Dry Van, Pick-up Delivery, Utility/Service, Beverage, Dump, Plow/Spreader, Refuse, Mixer, Bus, Wrecker, Heavy Haul, Forestry, Oil Field, Construction","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology ?????? Clutched Air Compressor\"","N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"International Motors, LLC","JNVX2TRACIXM","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACIXM-020","International 9900","Diesel","10 years / 435,000 mi","Y","N",72,54,95,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"N",null,"Y","Y","N","Y","2017-01-02","Vehicle speed limiter"]
[2018,"International Motors, LLC","JNVX2TRACIXL","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACIXL-019","International LT","Diesel","10 years / 435,000 mi","Y","N",73,63,86,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2017-01-02","Innovative technologies"]
[2018,"International Motors, LLC","JNVX2TRACXXL","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACXXL-023","International LoneStar","Diesel","10 years / 435,000 mi","Y","N",73,58,86,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXM","Y","Y",null,"Y","2017-01-02","Low rolling resistance tires"]
[2018,"International Motors, LLC","JNVX2TRACIXL","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACIXL-019","International LT","Diesel","10 years / 435,000 mi","Y","N",73,63,86,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2017-01-02","Low rolling resistance tires"]
[2018,"International Motors, LLC","JNVX2VOCVIXB","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","JNVX2VOCVIXB-005","International DuraStar","Diesel","10 years / 185,000 mi","Y","N",225,211,238,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"International Motors, LLC","JNVX2TRACXXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACXXK-024","RH","Diesel","10 years / 435,000 mi","Y","N",66,52,78,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXM","Y","Y",null,"Y","2017-01-02","Vehicle weight reduction"]
[2018,"Daimler Truck North America LLC","JDTN2VOCV17C","Class 8 vocational tractors","JDTN2VOCV17C-005","Freightliner SD Coronado","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"Pickup and Delivery/Short Haul Service Logging Service Oil Field Service Utility/Repair/Maintenance Service Construction Service Wrecking Service Farm Service Line Haul/Long Haul Service Mining Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC11C","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","JDTN2TRAC11C-011","Western Star 4700SB/4700SF","Diesel","10 years / 435,000 mi","Y","N",86,79,103,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC12C","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","JDTN2TRAC12C-012","Freightliner Coronado 122/132","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",73,72,98,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Refuse Service Heavy Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC14C","Y","Y",null,"Y","2017-01-02","Vehicle weight reduction"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JDTN2TRAC07C-007","Freightliner Cascadia 113/125","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",115,105,134,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC08C","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JDTN2TRAC08C-008","Freightliner M2 106/112","Diesel","10 years / 185,000 mi","Y","N",120,104,151,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","JPCR2TRAC8DM-006","Model 579","Compressed Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC8DH","Y","Y",null,"Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","JPCR2TRAC8DM-006","Model 386","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC8DH","Y","Y",null,"Y","2017-01-02","Gap reducing fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","JPCR2TRAC8DL-005","Model 348","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC8DH","Y","Y",null,"Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","JPCR2TRAC8DL-005","K500","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC8DH","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"PACCAR Inc","JPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JPCR2TRAC7DM-003","T680","Diesel","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC7DH","Y","Y",null,"Y","2017-01-02","Vehicle speed limiter"]
[2018,"PACCAR Inc","JPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JPCR2TRAC7DM-003","T370","Diesel","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC7DH","Y","Y",null,"Y","2017-01-02","Vehicle weight reduction"]
[2018,"PACCAR Inc","JPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JPCR2TRAC7DL-002","Model 520","Diesel","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC7DH","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"PACCAR Inc","JPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JPCR2TRAC7DL-002","T370","Compressed Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","JPCR2TRAC7DH","Y","Y",null,"Y","2017-01-02","Gap reducing fairing"]
[2018,"International Motors, LLC","JNVX2TRACIXG","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","JNVX2TRACIXG-016","International ProStar","Diesel","10 years / 435,000 mi","Y","N",80,68,85,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXJ","Y","Y","N","Y","2017-01-02","Gap reducing fairing"]
[2018,"International Motors, LLC","JNVX2VOCVIXB","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","JNVX2VOCVIXB-005","International TerraStar","Diesel","10 years / 185,000 mi","Y","N",225,211,238,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",{"$nulls":8},"2017-01-02","Innovative technologies"]
[2018,"International Motors, LLC","JNVX2VOCVIXB","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","JNVX2VOCVIXB-005","International Stripped Chassis (FBTC)","Diesel","10 years / 185,000 mi","Y","N",225,211,238,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"International Motors, LLC","JNVX2TRACIXE","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JNVX2TRACIXE-011","TranStar","Diesel","10 years / 185,000 mi","Y","N",115,108,123,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXF","Y","Y","N","Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"International Motors, LLC","JNVX2VOCVXXC","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","JNVX2VOCVXXC-002","International HV","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Dry Van, Pick-up Delivery, Utility/Service, Beverage, Dump, Plow/Spreader, Refuse, Mixer, Bus, Wrecker, Heavy Haul, Forestry, Oil Field, Construction","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"PACCAR Inc","JPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","JPCR2TRAC8DH-004","Model 389","Diesel","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","JPCR2TRAC8DH-004","T470","Diesel","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","JPCR2TRAC8DH-004","T660","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Vehicle speed limiter"]
[2018,"Daimler Truck North America LLC","JDTN2VOCV17C","Class 8 vocational tractors","JDTN2VOCV17C-005","Western Star 5700XE","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"Pickup and Delivery/Short Haul Service Logging Service Oil Field Service Utility/Repair/Maintenance Service Construction Service Wrecking Service Farm Service Line Haul/Long Haul Service Mining Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC13C","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","JDTN2TRAC13C-013","Western Star 4700SB/4700SF","Compressed Natural Gas","10 years / 435,000 mi","Y","N",89,79,115,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Low rolling resistance tires"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC11C","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","JDTN2TRAC11C-011","Western Star 4700SB/4700SF","Compressed Natural Gas","10 years / 435,000 mi","Y","N",86,79,103,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC10C","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","JDTN2TRAC10C-010","Freightliner Cascadia 116/126","Compressed Natural Gas","10 years / 435,000 mi","Y","N",66,64,89,"Line Haul/Long Haul Service Heavy Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Low rolling resistance tires"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC08C","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JDTN2TRAC08C-008","Freightliner M2 106/112","Compressed Natural Gas","10 years / 185,000 mi","Y","N",120,104,151,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Vehicle weight reduction"]
[2018,"Daimler Truck North America LLC","JDTN2TRAC06C","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JDTN2TRAC06C-006","Freightliner SD108/SD114/SD122","Diesel","10 years / 185,000 mi","Y","N",104,96,124,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2017-01-02","Low rolling resistance tires"]
[2018,"XOS, Inc.","JTHO2VOCV100","Class 8 vocational tractors","JTHO2VOCV100-001","ET1-600","Electricity","10 years / 435,000 mi","N","N",222,0,0,"Drayage and Regional Haul","N",null,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2018-01-01","Advanced technologies"]
[2018,"International Motors, LLC","JNVX2VOCVXXP","Class 8 vocational tractors","JNVX2VOCVXXP-004","International LS","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Heavy Hauler Tractor, On/Off Highway Tractor, Oil Field Tractor, Forestry Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"International Motors, LLC","JNVX2TRACXXJ","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","JNVX2TRACXXJ-017","International LoneStar","Diesel","10 years / 435,000 mi","Y","N",89,73,103,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Vehicle weight reduction"]
[2018,"International Motors, LLC","JNVX2TRACXXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACXXK-024","International 9900","Diesel","10 years / 435,000 mi","Y","N",66,52,78,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXM","Y","Y",null,"Y","2017-01-02","Gap reducing fairing"]
[2018,"PACCAR Inc","JPCR2VOCV8TK","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","JPCR2VOCV8TK-013","T880","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,203,237,"Construction, refuse, pickup and delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"PACCAR Inc","JPCR2VOCV8TK","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","JPCR2VOCV8TK-013","T680","Diesel","10 years / 435,000 mi","Y","N",222,203,237,"Construction, refuse, pickup and delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2017-01-02","Low rolling resistance tires"]
[2018,"PACCAR Inc","JPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","JPCR2TRAC8SM-009","T440","Compressed Natural Gas","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","JPCR2TRAC8SH","Y","Y",null,"Y","2017-01-02","Gap reducing fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8SL","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","JPCR2TRAC8SL-008","Model 587","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",66,47,79,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","JPCR2TRAC8SH","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","JPCR2TRAC8SH-007","K500","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","JPCR2TRAC8SH-007","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2017-01-02","Gap reducing fairing"]
[2018,"PACCAR Inc","JPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","JPCR2TRAC8SH-007","T660","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2017-01-02","Vehicle speed limiter"]
[2018,"International Motors, LLC","JNVX2TRACXXL","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","JNVX2TRACXXL-023","International 9900","Diesel","10 years / 435,000 mi","Y","N",73,58,86,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXM","Y","Y",null,"Y","2017-01-02","Aerodynamic roof fairing"]
[2018,"International Motors, LLC","JNVX2TRACXXD","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JNVX2TRACXXD-007","ProStar","Diesel","10 years / 185,000 mi","Y","N",104,88,113,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXF","Y","Y",null,"Y","2017-01-02","Low rolling resistance tires"]
[2018,"PACCAR Inc","JPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JPCR2TRAC7DH-001","Model 382","Compressed Natural Gas","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Low rolling resistance tires"]
[2018,"PACCAR Inc","JPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","JPCR2TRAC7DH-001","C500","Diesel","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2017-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"International Motors, LLC","HNVX2TRACXXE","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HNVX2TRACXXE-016","TranStar","Diesel","10 years / 185,000 mi","Y","N",115,108,123,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HNVX2TRACXXF","Y","Y",null,"Y","2016-01-02","Vehicle weight reduction"]
[2017,"International Motors, LLC","HNVX2TRACIXG","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HNVX2TRACIXG-023","9900","Diesel","10 years / 435,000 mi","Y","N",80,68,85,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXJ","Y","Y","N","Y","2016-01-02","Aerodynamic roof fairing"]
[2017,"International Motors, LLC","HNVX2TRACXXM","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACXXM-007","ProStar","Diesel","10 years / 435,000 mi","Y","N",72,54,95,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-02","Vehicle weight reduction"]
[2017,"International Motors, LLC","HNVX2TRACXXM","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACXXM-007","LT","Diesel","10 years / 435,000 mi","Y","N",72,54,95,"Tractors","Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"International Motors, LLC","HNVX2VOCVIXB","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HNVX2VOCVIXB-014","TranStar","Diesel","10 years / 185,000 mi","Y","N",225,211,238,"Dry Van, Pick-up/Delivery, Utility/Service, Dump, Plow/Spreader, Refuse, Flat Bed, Mixer, School Bus, Commercial Bus, RV, Step-Van, Wrecker","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",{"$nulls":8},"2016-01-02","Innovative technologies"]
[2017,"PACCAR Inc","HPCR2VOCV7TK","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2VOCV7TK-002","T470","Diesel","10 years / 185,000 mi","Y","N",225,205,241,"Construction, refuse, pickup and delivery, utility, snow plow, oil field, wrecker, fire/emergency, crane, agriculture, car hauler, regional haul","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DL-010","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DL-010","T470","Diesel","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","Model 320","Diesel","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","T370","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Vehicle weight reduction"]
[2017,"PACCAR Inc","HPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DM-014","Model 382","Compressed Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-28","Aerodynamic roof fairing"]
[2017,"PACCAR Inc","HPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DL-010","T660","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DL-010","T470","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DH-009","T370","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-28","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DH-009","Model 348","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-28","Vehicle weight reduction"]
[2017,"PACCAR Inc","HPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DM-012","Model 389","Compressed Natural Gas","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-28","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DM-012","C500","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-28","Aerodynamic roof fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","Model 579","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Gap reducing fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Aerodynamic roof fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DH-011","Model 348","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-28","Vehicle weight reduction"]
[2017,"International Motors, LLC","HNVX2TRACIXE","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HNVX2TRACIXE-021","TranStar","Diesel","10 years / 185,000 mi","Y","N",115,108,123,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXF","Y","Y","N","Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"International Motors, LLC","HNVX2VOCVIXC","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HNVX2VOCVIXC-003","TranStar","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Dry Van, Pick-up Delivery, Utility/Service, Beverage, Dump, Plow/Spreader, Refuse, Mixer, Bus, Wrecker, Heavy Haul, Forestry, Oil Field, Construction","Y",0,1,"N","N",{"$nulls":3},"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology â€“ Clutched Air Compressor\"","N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SM-007","Model 389","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","HPCR2TRAC8SH","Y","Y",null,"Y","2016-01-02","Aerodynamic roof fairing"]
[2017,"PACCAR Inc","HPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SM-007","T680","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","HPCR2TRAC8SH","Y","Y",null,"Y","2016-01-02","Automatic engine shutdown system"]
[2017,"Daimler Truck North America LLC","HDTN2TRAC13C","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","HDTN2TRAC13C-013","Freightliner Coronado 122/132","Compressed Natural Gas","10 years / 435,000 mi","Y","N",89,79,115,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"Daimler Truck North America LLC","HDTN2TRAC14C","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","HDTN2TRAC14C-014","Freightliner Coronado SD","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72,65,108,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-02","Vehicle weight reduction"]
[2017,"Daimler Truck North America LLC","HDTN2TRAC09C","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HDTN2TRAC09C-009","Western Star 4900EX/4900FA/4900SA","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,73,96,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service Heavy Haul Service Refuse Service Wrecking Service Utility/Repair/Maintenance Service Fire Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"Daimler Truck North America LLC","HDTN2TRAC07C","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2TRAC07C-007","Western Star 4900EX/4900FA/4900SA","Diesel","10 years / 185,000 mi","Y","N",115,105,134,"Line Haul/Long Haul Service Pickup and Delivery/Short Haul Service","N",null,1,"Y","N","N","N",null,"N",null,null,"N",null,null,"Y","HDTN2TRAC13C","Y","Y",null,"Y","2016-01-02","Vehicle weight reduction"]
[2017,"PACCAR Inc","HPCR2TRAC8SM","Class 8 mid-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SM-007","Model 365","Compressed Natural Gas","10 years / 435,000 mi","Y","N",73,52,88,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","HPCR2TRAC8SH","Y","Y",null,"Y","2016-01-02","Vehicle weight reduction"]
[2017,"PACCAR Inc","HPCR2TRAC8DM","Class 8 mid-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DM-014","T880","Compressed Natural Gas","10 years / 435,000 mi","Y","N",86,67,94,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-28","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SH-006","Model 587","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2016-01-02","Automatic engine shutdown system"]
[2017,"PACCAR Inc","HPCR2TRAC8SH","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SH-006","Model 384","Compressed Natural Gas","10 years / 435,000 mi","Y","N",72,48,97,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","N",null,"Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC8SL","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SL-008","Model 384","Diesel","10 years / 435,000 mi","Y","N",66,47,79,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","HPCR2TRAC8SH","Y","Y",null,"Y","2016-01-02","Automatic engine shutdown system"]
[2017,"PACCAR Inc","HPCR2TRAC8SL","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SL-008","T660","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",66,47,79,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","HPCR2TRAC8SH","Y","Y",null,"Y","2016-01-02","Automatic engine shutdown system"]
[2017,"PACCAR Inc","HPCR2TRAC8SL","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HPCR2TRAC8SL-008","Model 367","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",66,47,79,null,"Y",0,1,"N","Y","Y","Y","The engine will shutdown whenever the vehicle is stationary for 300s, the parking brake is set, and none of the following reset conditions have occurred: 1) Accelerator pedal has been actuated 2) Service brake pedal has been actuated 3) Clutch pedal has been actuated On Cummins-manufactured engine installations, (1) through (3) will reset the timer at any point. On PACCAR-manufactured engine installations, (1) through (3) will have no impact on the timer's behavior until the final 60s of the timer's countdown.","N",null,null,"N",null,"The AES system may be overridden by: 1) Any of the temperature conditions listed in the attached AECD 2) A DPF regeneration 3) While servicing the engine (see notes (a) & (b) below) a) Cummins-manufactured engines will only overrule the shutdown timer for the following tests: SCR Performance Test, Fuel Injector Performance Test b) PACCAR-manufactured engines will shut down and the AES overrule will be canceled when the PACCAR service tool has been disconnected from the vehicle and the engine has been shut off manually for sixty minutes or longer.","Y","HPCR2TRAC8SH","Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DL-010","963","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-02","Gap reducing fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DH","Class 7 high-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DH-011","T440","Compressed Natural Gas","10 years / 185,000 mi","Y","N",120,84,140,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-28","Gap reducing fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","Model 367","Diesel","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Gap reducing fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","Model 579","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DM-012","T880","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-28","Vehicle weight reduction"]
[2017,"PACCAR Inc","HPCR2TRAC7DM","Class 7 mid-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DM-012","T800","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",115,86,125,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-28","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DH-009","T800","Compressed Natural Gas","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-28","Vehicle weight reduction"]
[2017,"PACCAR Inc","HPCR2TRAC8DH","Class 8 high-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DH-009","Model 384","Diesel","10 years / 435,000 mi","Y","N",89,66,105,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"N",null,"Y","Y",null,"Y","2016-01-28","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2TRACIXM","Class 8 high-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXM-010","LoneStar","Diesel","10 years / 435,000 mi","Y","N",72,54,95,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"N",null,"Y","Y","N","Y","2016-01-02","Vehicle speed limiter"]
[2017,"PACCAR Inc","HPCR2VOCV8TK","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HPCR2VOCV8TK-004","Model 386","Diesel","10 years / 435,000 mi","Y","N",222,203,237,"Construction, refuse, pickup and delivery, utility, snow plow, mining, oil field, wrecker, regional haul, fire/emergency, crane, agriculture, car hauler","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2VOCV7TK","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2VOCV7TK-002","T800","Diesel","10 years / 185,000 mi","Y","N",225,205,241,"Construction, refuse, pickup and delivery, utility, snow plow, oil field, wrecker, fire/emergency, crane, agriculture, car hauler, regional haul","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC8DL","Class 8 low-roof day cab tractors above 33,000 pounds GVWR","HPCR2TRAC8DL-010","Model 384","Compressed Natural Gas","10 years / 435,000 mi","Y","N",80,63,87,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC8DH","Y","Y",null,"Y","2016-01-02","Low rolling resistance tires"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","Model 567","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"PACCAR Inc","HPCR2TRAC7DL","Class 7 low-roof tractors all cabs above 26,000 pounds GVWR and at or below 33,000 pounds GVWR","HPCR2TRAC7DL-013","Model 389","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",104,80,114,null,"Y",0,1,"N","N","Y","N",null,"N",null,null,"N",null,null,"Y","HPCR2TRAC7DH","Y","Y",null,"Y","2016-01-02","Gap reducing fairing"]
[2017,"Motor Coach Industries","HMCH2VOCVMCI","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HMCH2VOCVMCI-001","D 4000","Diesel","10 years / 435,000 mi","Y","N",222,209,220,"MOTOR COACH AND INMATE TRANSPORTATION VEHICLE","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-05-16","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Coronado 122/132","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Coronado 122/132","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Coronado 122/132","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner M2 106/112","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner M2 106/112","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner M2 106/112","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner M2 106/112","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XBA/XBP/XBR/XBS Chassis","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XBA/XBP/XBR/XBS Chassis","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XBA/XBP/XBR/XBS Chassis","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XBA/XBP/XBR/XBS Chassis","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XBA/XBP/XBR/XBS Chassis","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner SD Coronado","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner SD Coronado","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner SD Coronado","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner SD Coronado","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner SD Coronado","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4700SB/4700SF","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4700SB/4700SF","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4700SB/4700SF","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4700SB/4700SF","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4700SB/4700SF","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Cascadia 113/125","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Cascadia 113/125","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Cascadia 113/125","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Cascadia 113/125","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Freightliner Cascadia 113/125","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2VOCVXXP","Class 8 vocational tractors","HNVX2VOCVXXP-005","WorkStar","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Heavy Hauler Tractor, On/Off Highway Tractor, Oil Field Tractor, Forestry Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2VOCVXXP","Class 8 vocational tractors","HNVX2VOCVXXP-005","Cat CT660/CT670/CT680/CT681","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Heavy Hauler Tractor, On/Off Highway Tractor, Oil Field Tractor, Forestry Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2VOCVXXP","Class 8 vocational tractors","HNVX2VOCVXXP-005","DuraStar","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Heavy Hauler Tractor, On/Off Highway Tractor, Oil Field Tractor, Forestry Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2VOCVXXP","Class 8 vocational tractors","HNVX2VOCVXXP-005","Commercial Buses","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Heavy Hauler Tractor, On/Off Highway Tractor, Oil Field Tractor, Forestry Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2VOCVXXP","Class 8 vocational tractors","HNVX2VOCVXXP-005","HX Series","Diesel","10 years / 435,000 mi","Y","N",222,208,233,"Heavy Hauler Tractor, On/Off Highway Tractor, Oil Field Tractor, Forestry Tractor, End Dump Tractor, Construction Tractor, Low-roof Beverage or City Tractor","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","ProStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","ProStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Aerodynamic roof fairing"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","ProStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","ProStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Innovative technologies"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","ProStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Vehicle weight reduction"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","ProStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Vehicle speed limiter"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","ProStar","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Gap reducing fairing"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","9900","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Low rolling resistance tires"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","9900","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Aerodynamic roof fairing"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","9900","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Aerodynamic side skirt and/or fuel tank fairing"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","9900","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Innovative technologies"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","9900","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Vehicle weight reduction"]
[2017,"International Motors, LLC","HNVX2TRACIXK","Class 8 low-roof sleeper cab tractors above 33,000 pounds GVWR","HNVX2TRACIXK-011","9900","Diesel","10 years / 435,000 mi","Y","N",66,58,78,"Tractors","Y",0,1,"N","N","Y","N",null,"Y","Clutched Air Compressor","Document \"Navistar Innovative Technology - Clutched Air Compressor\"","N",null,null,"Y","HNVX2TRACXXM","Y","Y","N","Y","2016-01-02","Vehicle speed limiter"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","Freightliner M2 106","Liquid Petroleum Gas","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","Freightliner M2 106","Diesel","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","Freightliner M2 106","Gasoline (including gasoline blends up to E85)","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","Freightliner M2 106","Liquefied Natural Gas","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","Freightliner M2 106","Compressed Natural Gas","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","FCCC MBC/MC/MT45/MT55 Chassis","Liquid Petroleum Gas","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","FCCC MBC/MC/MT45/MT55 Chassis","Diesel","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","FCCC MBC/MC/MT45/MT55 Chassis","Gasoline (including gasoline blends up to E85)","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","FCCC MBC/MC/MT45/MT55 Chassis","Liquefied Natural Gas","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV03C","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","HDTN2VOCV03C-001","FCCC MBC/MC/MT45/MT55 Chassis","Compressed Natural Gas","10 years / 110,000 mi","Y","N",373,354,423,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency Service Utility/Repair/Maintenance Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner Cascadia 113/125","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner Cascadia 113/125","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner Cascadia 113/125","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner Cascadia 113/125","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner Cascadia 113/125","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XBA/XBP/XBR/XBS Chassis","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XBA/XBP/XBR/XBS Chassis","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XBA/XBP/XBR/XBS Chassis","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XBA/XBP/XBR/XBS Chassis","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XBA/XBP/XBR/XBS Chassis","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner M2 106/112","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner M2 106/112","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner M2 106/112","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner M2 106/112","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner M2 106/112","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC S2/SL/MB65/FRED Chassis","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC S2/SL/MB65/FRED Chassis","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC S2/SL/MB65/FRED Chassis","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC S2/SL/MB65/FRED Chassis","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC S2/SL/MB65/FRED Chassis","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Thomas Built Bus C2/EFX/HDX","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Thomas Built Bus C2/EFX/HDX","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Thomas Built Bus C2/EFX/HDX","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Thomas Built Bus C2/EFX/HDX","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Thomas Built Bus C2/EFX/HDX","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner SD108/SD114/SD122","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner SD108/SD114/SD122","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner SD108/SD114/SD122","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner SD108/SD114/SD122","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Freightliner SD108/SD114/SD122","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC XCL/XCM/XCP/XCR/XCS Chassis","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC MBC/MC/MT45/MT55 Chassis","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC MBC/MC/MT45/MT55 Chassis","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC MBC/MC/MT45/MT55 Chassis","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC MBC/MC/MT45/MT55 Chassis","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","FCCC MBC/MC/MT45/MT55 Chassis","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Western Star 4700SB/4700SF","Diesel","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Western Star 4700SB/4700SF","Compressed Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Western Star 4700SB/4700SF","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Western Star 4700SB/4700SF","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV04C","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","HDTN2VOCV04C-002","Western Star 4700SB/4700SF","Liquefied Natural Gas","10 years / 185,000 mi","Y","N",225,211,265,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC S2/SL/MB65/FRED Chassis","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC S2/SL/MB65/FRED Chassis","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC S2/SL/MB65/FRED Chassis","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC S2/SL/MB65/FRED Chassis","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","FCCC S2/SL/MB65/FRED Chassis","Liquefied Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4900EX/4900FA/4900SA","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4900EX/4900FA/4900SA","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4900EX/4900FA/4900SA","Diesel","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2017,"Daimler Truck North America LLC","HDTN2VOCV05C","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","HDTN2VOCV05C-003","Western Star 4900EX/4900FA/4900SA","Compressed Natural Gas","10 years / 435,000 mi","Y","N",222,208,260,"City Transit Bus Pickup and Delivery/Short Haul Service Recreation Service Rescue and Emergency / Fire Service Utility/Repair/Maintenance Service Construction Service Airport Service Farm Service Line Haul/Long Haul Service Mining Service Refuse Service School Bus Service Shuttle Bus Tour Bus/Coach - City Wrecking Service Church/Prison/Activity Bus Charter/Shuttle Transit Bus Service Mobile Lab Service","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-02","Low rolling resistance tires"]
[2016," BYD Auto Industry Company Limited","GBYD2VOCVK71","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBYD2VOCVK71-001","BYD Electric Bus 30ft","Electricity","10 years / 185,000 mi","N","N",234,0,0,"application for BYD Electric Bus 30ft","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2015-09-01","Advanced technologies"]
[2016,"GILLIG LLC","GGLG2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GGLG2VOCVHHD-002","LOWFLOOR","Diesel","10 years / 435,000 mi","Y","N",226,212,238,"TRANSIT BUS","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-01","Low rolling resistance tires"]
[2016,"GILLIG LLC","GGLG2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GGLG2VOCVMHD-001","Lowfloor","Diesel","10 years / 185,000 mi","Y","N",234,219,247,"transit bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-01","Low rolling resistance tires"]
[2016," BYD Auto Industry Company Limited","GBYD2VOCVT51","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GBYD2VOCVT51-003","BYD T5","Electricity","10 years / 110,000 mi","N","N",388,0,0,"application for BYD T5","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2015-12-01","Advanced technologies"]
[2016," BYD Auto Industry Company Limited","GBYD2VOCVT91","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBYD2VOCVT91-005","BYD T9","Electricity","10 years / 435,000 mi","N","N",226,0,0,"application for BYD T9","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2015-12-31","Advanced technologies"]
[2016," BYD Auto Industry Company Limited","GBYD2VOCVT71","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBYD2VOCVT71-004","BYD T7","Electricity","10 years / 185,000 mi","N","N",234,0,0,"application for BYD T7","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2015-12-31","Advanced technologies"]
[2016," BYD Auto Industry Company Limited","GBYD2VOCVK11","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBYD2VOCVK11-007-R01","BYD Electric Bus 60ft","Electricity","10 years / 435,000 mi","N","N",226,0,0,"application for BYD Electric Bus 60ft","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2015-12-01","Advanced technologies"]
[2016,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","GVPT2VOCVE00","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GVPT2VOCVE00-001","Nova Bus LFS, LFS Artic","Diesel","10 years / 435,000 mi","Y","N",226,207,244,"urban and regional transit buses","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-15","Low rolling resistance tires"]
[2016,"Volvo Group Trucks Technology, Powertrain Engineering, a Division of Mack Trucks","GVPT2VOCVE00","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GVPT2VOCVE00-001","Nova Bus LFX","Diesel","10 years / 435,000 mi","Y","N",226,207,244,"urban and regional transit buses","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-15","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Diesel","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Diesel","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Diesel","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Diesel","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","EZRIDER II HYBRID DIESEL","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","EZRIDER II HYBRID DIESEL","Electricity","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","EZRIDER II HYBRID DIESEL","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","EZRIDER II DIESEL","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","EZRIDER II DIESEL","Electricity","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","EZRIDER II DIESEL","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","XHF DIESEL","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","XHF DIESEL","Electricity","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","XHF DIESEL","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS FUELCELL","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS FUELCELL","Electricity","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS FUELCELL","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS ELECTRIC","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS ELECTRIC","Electricity","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS ELECTRIC","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS DIESEL","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS DIESEL","Electricity","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS DIESEL","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS HYBRID DIESEL","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS HYBRID DIESEL","Electricity","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV001-001","AXESS HYBRID DIESEL","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Dennis Eagle Inc","GDEI2VOCVCOL","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GDEI2VOCVCOL-001","DENNIS EAGLE, INC.","Diesel","10 years / 435,000 mi","N","N",226,216,216,"Model Year 2016 Application for Certification for HHDV vehicle  for Dennis Eagle, Inc.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-03-22","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Diesel","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Diesel","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Diesel","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Diesel","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016," BYD Auto Industry Company Limited","GBYD2VOCVK91","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBYD2VOCVK91-002-R01","BYD Electric Bus 40ft","Electricity","10 years / 435,000 mi","N","N",226,0,0,"application for BYD Electric Bus 40ft","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2015-12-01","Advanced technologies"]
[2016,"New Flyer of America Inc.","GNFA2VOCV002","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GNFA2VOCV002-002","New Flyer MiDi","Diesel","10 years / 185,000 mi","Y","N",234,228,228,"Medium Duty City Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-01","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV002","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV002-002","EZRIDER II CNG","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV002","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV002-002","XHF CNG","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV002","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV002-002","AXESS CNG","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV003","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GEDR2VOCV003-003","TRANSMARK RE","Diesel","10 years / 185,000 mi","Y","N",234,215,240,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV003","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GEDR2VOCV003-003","UK PROJECT","Diesel","10 years / 185,000 mi","Y","N",234,215,240,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV003","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GEDR2VOCV003-003","EZRIDER II DIESEL","Diesel","10 years / 185,000 mi","Y","N",234,215,240,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-18","Low rolling resistance tires"]
[2016,"General Motors LLC","GGMX2VOCVTIR","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GGMX2VOCVTIR-001","Chevrolet Express Cutaway Chassis","Diesel","10 years / 110,000 mi","Y","N",388,381,386,"Vocational Vehicle","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-04-12","Low rolling resistance tires"]
[2016,"General Motors LLC","GGMX2VOCVTIR","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GGMX2VOCVTIR-001","Chevrolet Express Cargo 2WD","Diesel","10 years / 110,000 mi","Y","N",388,381,386,"Vocational Vehicle","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-04-12","Low rolling resistance tires"]
[2016,"General Motors LLC","GGMX2VOCVTIR","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GGMX2VOCVTIR-001","Chevrolet Express Pass. 2WD","Diesel","10 years / 110,000 mi","Y","N",388,381,386,"Vocational Vehicle","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-04-12","Low rolling resistance tires"]
[2016,"General Motors LLC","GGMX2VOCVTIR","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GGMX2VOCVTIR-001","GMC Savana Cutaway Chassis","Diesel","10 years / 110,000 mi","Y","N",388,381,386,"Vocational Vehicle","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-04-12","Low rolling resistance tires"]
[2016,"General Motors LLC","GGMX2VOCVTIR","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GGMX2VOCVTIR-001","GMC Savana Cargo 2WD","Diesel","10 years / 110,000 mi","Y","N",388,381,386,"Vocational Vehicle","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-04-12","Low rolling resistance tires"]
[2016,"General Motors LLC","GGMX2VOCVTIR","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GGMX2VOCVTIR-001","GMC Savana Pass. 2WD","Diesel","10 years / 110,000 mi","Y","N",388,381,386,"Vocational Vehicle","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-04-12","Low rolling resistance tires"]
[2016,"Kovatch Mobile Equipment Corporation","GKME2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GKME2VOCV001-001","Rescue","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"This family is made up of standard pumper, rescue, tanker, and aerial vehicles for fire rescue operations.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-05-06","Low rolling resistance tires"]
[2016,"Kovatch Mobile Equipment Corporation","GKME2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GKME2VOCV001-001","Pumper","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"This family is made up of standard pumper, rescue, tanker, and aerial vehicles for fire rescue operations.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-05-06","Low rolling resistance tires"]
[2016,"Kovatch Mobile Equipment Corporation","GKME2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GKME2VOCV001-001","Aerial","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"This family is made up of standard pumper, rescue, tanker, and aerial vehicles for fire rescue operations.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-05-06","Low rolling resistance tires"]
[2016,"Kovatch Mobile Equipment Corporation","GKME2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GKME2VOCV001-001","Tanker","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"This family is made up of standard pumper, rescue, tanker, and aerial vehicles for fire rescue operations.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-05-06","Low rolling resistance tires"]
[2016," BYD Auto Industry Company Limited","GBYD2VOCVK81","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBYD2VOCVK81-006","BYD Electric Bus 35ft","Electricity","10 years / 435,000 mi","N","N",226,0,0,"application for BYD Electric Bus 35ft","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"Y","Electric Vehicle",{"$nulls":7},"2015-12-01","Advanced technologies"]
[2016,"New Flyer of America Inc.","GNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GNFA2VOCV001-001","New Flyer Xcelsior","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,219,221,"Heavy Duty City Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-01","Low rolling resistance tires"]
[2016,"New Flyer of America Inc.","GNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GNFA2VOCV001-001","New Flyer Xcelsior","Diesel","10 years / 435,000 mi","Y","N",226,219,221,"Heavy Duty City Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-01-01","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD4000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FDB7000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD5000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex T500","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD6000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FDB4000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FDB6000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex T300","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD3000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"E-ONE, INC.","GENE2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GENE2VOCV001-001","Tanker","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"This family is made up of standard pumper trucks and tanker trucks for fire rescue.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-31","Low rolling resistance tires"]
[2016,"E-ONE, INC.","GENE2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GENE2VOCV001-001","Pumper","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"This family is made up of standard pumper trucks and tanker trucks for fire rescue.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-31","Low rolling resistance tires"]
[2016,"E-ONE, INC.","GENE2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GENE2VOCV001-001","Aerial","Diesel","10 years / 435,000 mi","Y","N",226,213,233,"This family is made up of standard pumper trucks and tanker trucks for fire rescue.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-12-31","Low rolling resistance tires"]
[2016,"Eldorado National-California Inc.","GEDR2VOCV004","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GEDR2VOCV004-004","AXESS FUEL CELL","Hydrogen","10 years / 435,000 mi","Y","N",226,213,233,"OVER THE ROAD - TRANSIT, SHUTTLE AND COMMUTER BUS.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-21","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FDB4000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex T500","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD6000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD4000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FDB6000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD5000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FDB7000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex T300","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Terex Corporation","GTRX2VOCVLRR","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GTRX2VOCVLRR-001","Terex FD3000","Diesel","10 years / 435,000 mi","Y","N",226,217,227,"Terex Corporation Heavy Heavy-Duty - Vocational Truck (Class 8) Front Discharge Concrete Mixer Truck and Truck Crane certification.  EPA / NHTSA Greenhouse Gas Standards Information- Terex is an EPA certified manufacturer of heavy duty highway vocational vehicles including Concrete Mixers and Truck Cranes.  All new Terex Concrete Mixers and Truck Cranes use LRR tires on both the steering axle and drive axles in order to fully comply with the applicable EPA GHG Emissions standards.","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-06-09","Low rolling resistance tires"]
[2016,"Alexander Dennis Limited","GADL2VOCV001","Class 8 vocational tractors","GADL2VOCV001-001","Enviro 400 (E400)","Diesel","10 years / 435,000 mi","N","N",226,215,221,"Urban bus services Transit bus services Inter-urban coach services","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-07-05","Vehicle speed limiter"]
[2016,"Alexander Dennis Limited","GADL2VOCV001","Class 8 vocational tractors","GADL2VOCV001-001","Enviro 500 (E500)","Diesel","10 years / 435,000 mi","N","N",226,215,221,"Urban bus services Transit bus services Inter-urban coach services","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-07-05","Vehicle speed limiter"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Diesel","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","All American","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Compressed Natural Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Diesel","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Liquid Petroleum Gas","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVMHD","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","GBBB2VOCVMHD-001-R01","Vision","Gasoline (including gasoline blends up to E85)","10 years / 185,000 mi","Y","N",234,219,236,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Diesel","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","Vision","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Diesel","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Gasoline (including gasoline blends up to E85)","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"Blue Bird Body Company","GBBB2VOCVHHD","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","GBBB2VOCVHHD-002-R01","All American","Liquid Petroleum Gas","10 years / 435,000 mi","Y","N",226,212,228,"Bus, School Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2016-10-24","Low rolling resistance tires"]
[2016,"FCA US LLC","GCRX2VOCV067","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GCRX2VOCV067-001","RAM 5500 CAB CHASSIS","Diesel","10 years / 110,000 mi","Y","N",388,381,389,"REQUEST FOR VEHICLE CoC Vocational Vehicles","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-07-31","Low rolling resistance tires"]
[2016,"FCA US LLC","GCRX2VOCV067","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GCRX2VOCV067-001","RAM 3500 CAB CHASSIS","Diesel","10 years / 110,000 mi","Y","N",388,381,389,"REQUEST FOR VEHICLE CoC Vocational Vehicles","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-07-31","Low rolling resistance tires"]
[2016,"FCA US LLC","GCRX2VOCV067","Class 2b-5 vocational vehicles at or below 19,500 pounds GVWR","GCRX2VOCV067-001","RAM 4500 CAB CHASSIS","Diesel","10 years / 110,000 mi","Y","N",388,381,389,"REQUEST FOR VEHICLE CoC Vocational Vehicles","N",null,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-07-31","Low rolling resistance tires"]
[2015,"New Flyer of America Inc.","FNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","FNFA2VOCV001-001","NABI BRT","Diesel","10 years / 435,000 mi","Y","N",226,214,227,"Heavy Duty Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-01-01","Low rolling resistance tires"]
[2015,"New Flyer of America Inc.","FNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","FNFA2VOCV001-001","NABI BRT","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,214,227,"Heavy Duty Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-01-01","Low rolling resistance tires"]
[2015,"New Flyer of America Inc.","FNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","FNFA2VOCV001-001","NABI LFW","Diesel","10 years / 435,000 mi","Y","N",226,214,227,"Heavy Duty Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-01-01","Low rolling resistance tires"]
[2015,"IRIZAR SOCIEDAD COOPERATIVA","FISV2VOCVIR1","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","FISV2VOCVIR1-001","IRIZAR i6","Diesel","10 years / 435,000 mi","N","N",226,213,213,"BUSES, MEDIUM AND LONG DISTANCE","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-10-01","Low rolling resistance tires"]
[2015,"New Flyer of America Inc.","FNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","FNFA2VOCV001-001","New Flyer Xcelsior","Diesel","10 years / 435,000 mi","Y","N",226,214,227,"Heavy Duty Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-01-01","Low rolling resistance tires"]
[2015,"New Flyer of America Inc.","FNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","FNFA2VOCV001-001","New Flyer Xcelsior","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,214,227,"Heavy Duty Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-01-01","Low rolling resistance tires"]
[2015,"New Flyer of America Inc.","FNFA2VOCV002","Class 6-7 vocational vehicles (other than vocational tractors) above 19,500 pounds GVWR and at or below 33,000 pounds GVWR","FNFA2VOCV002-002","New Flyer MiDi","Diesel","10 years / 185,000 mi","Y","N",234,228,228,"Medium Duty Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-01-01","Low rolling resistance tires"]
[2015,"New Flyer of America Inc.","FNFA2VOCV001","Class 8 vocational vehicles (other than vocational tractors) above 33,000 pounds GVWR","FNFA2VOCV001-001","NABI LFW","Compressed Natural Gas","10 years / 435,000 mi","Y","N",226,214,227,"Heavy Duty Transit Bus","Y",0,1,"N","N",{"$nulls":3},"N",null,null,"N",{"$nulls":8},"2015-01-01","Low rolling resistance tires"]

{"sheet":"ESRI_MAPINFO_SHEET","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}