{"text_format":"3","workbook":"xlsx","n_sheets":7,"sheets":["Cover Page","Table of Contents","Summary","Raw data","Surface water","Groundwater","Ambient air"],"not_rendered":{"images":1,"external_links":4,"defined_names":87},"read":"whole","date_system":"1900"}

{"sheet":"Cover Page","index":0,"n_rows":8,"n_cols":2,"rows_kept":8}
[]
[null,"PUBLIC RELEASE DRAFT"]
[null,"November 2024"]
[]
[null,"Draft Water Quality Portal (WQP) Monitoring Data 2011 to 2023 for 1,3-Butadiene"]
[]
[]
[null,"CASRN 106-99-0"]

{"sheet":"Table of Contents","index":1,"n_rows":10,"n_cols":2,"rows_kept":10,"merged":[[1,0,1,1]]}
["Description of this exposure and risk estimate workbook "]
["This workbook contains a summary of environmental concentrations collected from the WQP-Water Quality Portal. Data for 1,3-butadiene for the years 2011-2023 were downloaded from https://www.waterqualitydata.us, filtered to contain only data for 1,3-butadiene and exported to this file. This file contains sheets with the raw 1,3-butadiene data, a summary of the data in surface water, groundwater and ambient air, and individual sheets for surface water, groundwater and ambient air."]
[]
[]
["Worksheet","Description"]
["1,3-butadiene raw data","This tab provides the raw data for 1,3-butadiene from the WQP for the years 2011-2023. "]
["Summary","This tab provides a summary of the 1,3-butadiene data in surface water, groundwater and ambient air"]
["Surface Water","This tab provides the raw data filtered out to show surface water data (100% non-detects). The sample concentrations were assumed to be half the MDL. Note that two columns (CA and CB) were added to the data to calculate the assumed , mean and median concentrations of the samples."]
["Groundwater","This tab provides the raw data filtered out to show groundwater data detects (1% detects). The sample detects were used to compute the statistics. Note that two columns (AR and AS) were added to the data to calculate the mean and median concentrations of the measured samples. The MDL range is based on the MDL for non-detects since MDLs were not recorded for samples with measured concentrations of 1,3-butadiene in groundwater. "]
["Ambient Air","This tab provides the raw data filtered out to show ambient air data (100% non-detects). The sample concentrations were assumed to be half the MDL. Note that two columns (CA and CB) were added to the data to calculate the assumed, mean and median concentrations of the samples."]

{"sheet":"Summary","index":2,"n_rows":10,"n_cols":6,"rows_kept":10,"merged":[[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[3,1,9,1]]}
[]
[null,"Chemical","Statistics","Groundwater (µg/L)","Surface Water (µg/L)","Ambient Air "]
[{"$nulls":5},"(ppb)"]
[null,"1,3-Butadiene","Maximum",40,0.04,36]
[null,null,"Mean",2.52,0.04,6.88]
[null,null,"Median",2,0.04,2.6]
[null,null,"Minimum",2,0.04,0.37]
[null,null,"Total Samples",9378,231,25]
[null,null,"Total NDs","9288 (99%)","231 (100%)","25 (100%)"]
[null,null,"MDL","0.000299-2000",0.08,"0.74-72"]

{"sheet":"Raw data","index":3,"n_rows":10207,"n_cols":81,"rows_kept":1125,"cut":true,"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
["OrganizationIdentifier","OrganizationFormalName","ActivityIdentifier","ActivityTypeCode","ActivityMediaName","ActivityMediaSubdivisionName","ActivityStartDate","ActivityStartTime/Time","ActivityStartTime/TimeZoneCode","ActivityEndDate","ActivityEndTime/Time","ActivityEndTime/TimeZoneCode","ActivityRelativeDepthName","ActivityDepthHeightMeasure/MeasureValue","ActivityDepthHeightMeasure/MeasureUnitCode","ActivityDepthAltitudeReferencePointText","ActivityTopDepthHeightMeasure/MeasureValue","ActivityTopDepthHeightMeasure/MeasureUnitCode","ActivityBottomDepthHeightMeasure/MeasureValue","ActivityBottomDepthHeightMeasure/MeasureUnitCode","ProjectIdentifier","ProjectName","ActivityConductingOrganizationText","MonitoringLocationIdentifier","MonitoringLocationName","ActivityCommentText","SampleAquifer","HydrologicCondition","HydrologicEvent","ActivityLocation/LatitudeMeasure","ActivityLocation/LongitudeMeasure","SampleCollectionMethod/MethodIdentifier","SampleCollectionMethod/MethodIdentifierContext","SampleCollectionMethod/MethodName","SampleCollectionMethod/MethodDescriptionText","SampleCollectionEquipmentName","ResultIdentifier","ResultDetectionConditionText","MethodSpeciationName","CharacteristicName","ResultSampleFractionText","ResultMeasureValue","ResultMeasure/MeasureUnitCode","MeasureQualifierCode","ResultStatusIdentifier","StatisticalBaseCode","ResultValueTypeName","ResultWeightBasisText","ResultTimeBasisText","ResultTemperatureBasisText","ResultParticleSizeBasisText","DataQuality/PrecisionValue","DataQuality/BiasValue","DataQuality/ConfidenceIntervalValue","DataQuality/UpperConfidenceLimitValue","DataQuality/LowerConfidenceLimitValue","ResultCommentText","USGSPCode","ResultDepthHeightMeasure/MeasureValue","ResultDepthHeightMeasure/MeasureUnitCode","ResultDepthAltitudeReferencePointText","SubjectTaxonomicName","SampleTissueAnatomyName","BinaryObjectFileName","BinaryObjectFileTypeCode","ResultFileUrl","ResultAnalyticalMethod/MethodIdentifier","ResultAnalyticalMethod/MethodIdentifierContext","ResultAnalyticalMethod/MethodName","ResultAnalyticalMethod/MethodUrl","ResultAnalyticalMethod/MethodDescriptionText","LaboratoryName","AnalysisStartDate","ResultLaboratoryCommentText","ResultDetectionQuantitationLimitUrl","DetectionQuantitationLimitTypeName","DetectionQuantitationLimitMeasure/MeasureValue","DetectionQuantitationLimitMeasure/MeasureUnitCode","LabSamplePreparationUrl","LastUpdated","ProviderName"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303448","Sample-Routine","Water","Surface Water","2012-11-19","10:25:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05485605",null,"L-3250012 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 101000  per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-OK","USGS Oklahoma Water Science Center","nwisok.01.01300353","Sample-Routine","Water","Surface Water","2012-11-28","11:37:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-07159735",null,"L-3340023 LC8285 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107222450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301736","Sample-Routine","Water","Surface Water","2012-12-05","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05373005",null,"L-3420030 X = LC8252 deleted per request from WSC Bode, PG, 12/7/12   Received December 06, 2012  Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235052","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300359","Sample-Routine","Water","Surface Water","2012-11-28","11:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01391100",null,"L-3340075 LC8252 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01306829","Sample-Routine","Water","Surface Water","2012-12-11","12:40:00","MST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394847104570700",null,"L-3470006 Updated time from 1230 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107243373","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303140","Sample-Routine","Water","Surface Water","2012-12-04","12:10:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-08057410",null,"L-3400056 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301741","Sample-Routine","Water","Surface Water","2012-12-04","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05340041",null,"L-3400039 Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235727","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01303146","Sample-Routine","Water","Surface Water","2012-11-19","13:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01421640",null,"L-3250019 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 133000 per Romanok.  KB 05/13/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107213401","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300361","Sample-Routine","Water","Surface Water","2012-12-10","12:10:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01409480",null,"L-3460046 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302227","Sample-Routine","Water","Groundwater","2013-09-12","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325858082480101",null,"L-2590039 X = PHARM is not a GCV, it's a PHARM   Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  FUS btl type, smpl sent to WHOI without ASR, ASR recvd 10/29/13, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305560","Sample-Routine","Water","Groundwater","2013-07-10","09:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-350206118082401",null,"L-1920075 X = DOC is not a GCC please correct your labels..  S2437 split to 20131920165, paa, 2/19/14",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94953318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301075","Sample-Routine","Water","Groundwater","2013-09-05","14:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345927078170301",null,"L-2490157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96380393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306346","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364300119400001",null,"L-2420367 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96373953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400096","Quality Control Sample-Field Replicate","Water","Groundwater","2013-12-10","11:00:00","CST",{"$nulls":13},"USGS - Minnesota Water Science Center","MN040-450655093244701",null,"L-3450050 Added agency code per Langer.  KB 02/13/14  Samples were received chilled at the WHOI lab.  Added agency code per Langer.  KB 8/13/14",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-97038996","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300295","Sample-Routine","Water","Groundwater","2013-09-12","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405817117425401",null,"L-2560044 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96537369","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300200","Sample-Routine","Water","Groundwater","2013-08-13","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333036081442108",null,"L-2270106 Received August 14, 2013  LC1792 corrected to Scgedule 1792, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1100..  time added to ASR per radon, paa, 8/15/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95650577","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300791","Sample-Routine","Water","Groundwater","2013-08-21","14:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382825075081601",null,"A-2350143 3 drops HCl in VOC's",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104233375","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300982","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",173,"feet",208,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-421600085350001",null,"L-2420481 Received August 31, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Updated agency code from 0 to USGS per Beeler.  KB 01/21/14","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96406756","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302622","Sample-Routine","Water","Groundwater","2013-08-28","11:20:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-412307091031601",null,"L-2410170 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96416767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01304485","Sample-Routine","Water","Groundwater","2013-08-27","12:00:00","MDT",{"$nulls":4},4.95,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-402104104404501",null,"A-2420473 3 drops HCl each for schedules 4436 and 4437","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96352943","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301151","Sample-Routine","Water","Groundwater","2013-09-10","16:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345941078105001",null,"L-2550057 1 bottle leaked, 1/4 sample missing, per TAL   ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96444849","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300810","Sample-Routine","Water","Groundwater","2013-08-26","13:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382403075233201",null,"L-2400035 Received August 27, 2013",null,"Not applicable","Routine sample",null,null,4044,"USGS parameter code 82398","Submersible jet pump",null,"Submersible positive-pressure pump","NWIS-96270095","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300818","Sample-Routine","Water","Groundwater","2013-08-28","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390505075353901",null,"A-2410207 2 drops HCl in VOCs",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104234663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306550","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420003",null,"L-2630079 Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.  X = Time on sample 1001. Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible positive-pressure pump","NWIS-96557211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306408","Sample-Routine","Water","Groundwater","2013-09-11","09:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364600119460002",null,"L-2590041 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96466782","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302189","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-314733085071401",null,"L-2690200 Radon LC1369 removed from this ASR by Login, customer should do the same, paa, 10/24/13  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96617213","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305583","Sample-Routine","Water","Groundwater","2013-07-18","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363645119420901",null,"L-2060065 X = 2 empty GCVs - logged from problem cooler,relabeled remaining GCVs,paa,7/25/13    Received July 19,2013..  S2437 split to 20132060192, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94984590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303635","Sample-Routine","Water","Groundwater","2013-08-21","12:50:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-440354088560701",null,"L-2380159 Received August 23,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113295181","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302557","Sample-Routine","Water","Groundwater","2013-08-19","12:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-420158093562001",null,"L-2380248 logged from problem cooler, GCVs and PHARM missing date and time, paa added, WSC notified, paa, 8/26/13  Samples were received chilled at the WHOI lab.  logged from problem cooler, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95679036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400463","Quality Control Sample-Field Replicate","Water","Groundwater","2013-12-12","10:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370500120250001",null,"L-3470071 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106778047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305546","Sample-Routine","Water","Groundwater","2013-07-08","12:50:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-381100121200501",null,"L-1900067 S2437 split to 20131900098, paa, 2/19/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94889338","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300162","Sample-Routine","Water","Groundwater","2013-05-06","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392726119460101",null,"L-1280032 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131280085, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94501761","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306400","Sample-Routine","Water","Groundwater","2013-09-10","10:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364316119360801",null,"L-2540014 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-112097888","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300815","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382906075215101",null,"A-2400162 2 drops HCl in VOCs  Sample for Sch 1792",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96270551","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01300822","Sample-Routine","Water","Groundwater","2013-08-21","12:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420410111490401",null,"L-2350034 Received August 22, 2013    per Sue changed state and county codes  pwg  2013/09/16   Updated UC from UT per Masbruch.  KB 09/19/13..  Sta ID changed from 420410111490501 to 420410111490401 per Thiros, paa, 12/31/13  Samples were received chilled at the WHOI lab.   per Sue changed state an",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104187844","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301280","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303501087174801",null,"L-2610137 Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96718520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WV","USGS West Virginia Water Science Center","nwiswv.01.01300175","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393418078132201",null,"L-2330053 User Code VA changed to WV per A. Melberg, paa, 9/10/13  Begin date is missing in mandatory field, time = 1100, JNV  Samples were received chilled at the WHOI lab...  date added to ASR per NWQL ASRs, paa, 9/3/13..  User Code VA changed to WV per A. Melberg, paa, 9/10/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96337686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302223","Sample-Routine","Water","Groundwater","2013-09-16","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323842083393201",null,"L-2600160 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300051","Sample-Routine","Water","Groundwater","2013-06-25","14:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-343817079353709",null,"L-1770065 S2437 split to 20131770134, paa, 2/18/14  Corrected invalid LC1792 to Sch1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94764758","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300739","Sample-Routine","Water","Groundwater","2013-08-14","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390217076181401",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95458314","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300873","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","EDT",{"$nulls":6},"Below land-surface datum",270,"feet",280,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380147076351201",null,"L-2620149 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96501873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306542","Sample-Routine","Water","Groundwater","2013-09-18","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363700119590001",null,"L-2630166 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300196","Sample-Routine","Water","Groundwater","2013-08-28","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351113089513401",null,"A-2410226 2 drops HCl added to VOCs  Actual radon sample collection time: 1245 CDT (estimated + 30minutes) L-2410226 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96508627","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301210","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","CDT",{"$nulls":4},92,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-412538089215801",null,"L-2400205 Date & time added to ASR per btls, paa, 8/28/13  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96070182","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305615","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364356119374001",null,"L-2070169 PEST split to separate ASR @0931, paa 7/26/13  Received July 25, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95228768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306395","Sample-Routine","Water","Groundwater","2013-09-09","13:50:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364316119360101",null,"L-2540016 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96466310","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400292","Sample-Routine","Water","Groundwater","2013-12-03","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500119590001",null,"L-3380016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306537","Sample-Routine","Water","Groundwater","2013-09-16","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363100120050002",null,"L-2610093 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098446","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303380","Sample-Routine","Water","Groundwater","2013-07-31","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-453247088425701",null,"L-2130212 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113285583","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302857","Sample-Routine","Water","Groundwater","2013-09-03","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304603094101801",null,"L-2470133 Updated STAID from 304303094101701 as per Patty 10.23.14 MKS.  btl type is FUS, paa Samples were received chilled at the WHOI lab.  per Ging changed station id from 304303094101701   pwg  2013/09/07",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96436969","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301147","Sample-Routine","Water","Groundwater","2013-09-09","12:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345005078493601",null,"L-2550061 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300824","Sample-Routine","Water","Groundwater","2013-08-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-380022079025601",null,"L-2390043 Btl type for 2255 is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96294530","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305557","Sample-Routine","Water","Groundwater","2013-07-11","08:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-353833117424001",null,"L-1960027 Received Jul 12, 2013..  S2437 split to 20131960099, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94952873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302931","Sample-Routine","Water","Groundwater","2013-07-09","10:00:00","MDT",{"$nulls":4},21,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-410251102024201",null,"L-1930027 Received Jul 11, 2013..  S2437 split to 20131930237, paa, 2/20/14",null,"Not applicable","Routine sample",null,null,4080,"USGS parameter code 82398","Peristaltic pump",null,"Peristaltic pump","NWIS-94914690","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300321","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300719092294901",null,"L-2260165 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95515272","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300673","Sample-Routine","Water","Groundwater","2013-06-13","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",377,"feet",412,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312952089444201",null,"L-1650003 S2437 split to 20131650193, paa, 2/14/14  Field alk added per manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94718189","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302856","Sample-Routine","Water","Groundwater","2013-09-04","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305947093395001",null,"L-2480032 FA condition changed to improper preservation, JNV   Lab acidification lab code 3105 added, JNV   FA preserved by C.harris on 9/11/13 @ 10:38, JNV  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301259","Sample-Routine","Water","Groundwater","2013-09-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361224076514501",null,"L-2690094 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96580242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303070","Sample-Routine","Water","Groundwater","2013-09-12","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-281433097191300",null,"L-2560186 X = 1 4437 recvd broken GCV   Updated SID from 281418097193901 per Ging.  KB 8/5/14  ASRs recvd late & entered 1/21/14, paa   Updated SID from 281418097193901 per Ging.  KB 8/20/14  Updated SID from 281418097193901 per Ging.  KB 8/5/14  btl type is FUS, paa Samples were received chilled at",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96922915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300056","Sample-Routine","Water","Groundwater","2013-07-02","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352613088381501",null,"A-1860092 2 drops of HCl in VOCs  Actual radon collection time: 1325 L-1860092 S2437 split to 20131860105, paa, 2/19/14  Samples were received chilled at the WHOI lab.","McNairy Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95009041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306409","Sample-Routine","Water","Groundwater","2013-09-11","13:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364400119450002",null,"L-2590043 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-112098073","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01303480","Sample-Routine","Water","Groundwater","2013-07-30","11:30:00","MDT",{"$nulls":4},39,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-401544103443101",null,"A-2140130 5 drops HCl each for schedules 4436 and 4437","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95388806","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303412","Sample-Routine","Water","Groundwater","2013-08-14","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-433136089235301",null,"L-2270168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113289140","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300049","Sample-Routine","Water","Groundwater","2013-06-24","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-340823079514509",null,"L-1760159 S2437 split to 20131760221, paa, 2/18/14  Corrected invalid LC1792 to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94764296","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306341","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-29","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363700119550001",null,"L-2420364 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112097698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01301828","Sample-Routine","Water","Groundwater","2013-09-23","12:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392322094214601",null,"A-2670053 VOC's HAVE 3 DROPS HCL EACH VIAL  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres.  w/2mL NITRIC ACID <pH2  RADON SAMPL   (Mailed in Fed-Ex Box) alone   Sampled @ 1440",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96605644","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300438","Sample-Routine","Water","Groundwater","2013-08-28","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301312093094101",null,"L-2410172 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96361016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300729","Sample-Routine","Water","Groundwater","2013-07-23","08:30:00","CDT",{"$nulls":6},"Below land-surface datum",358,"feet",400,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-340658088425101",null,"L-2060078 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95323181","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300690","Sample-Routine","Water","Groundwater","2013-07-17","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-391832075560801",null,"L-2040031 Received July 19, 2013..  S2437 split to 20132040231, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94987707","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300106","Sample-Routine","Water","Groundwater","2013-08-07","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-331822081020809",null,"L-2210179 Received August 08, 2013  Corrected invalid LC1792 to schedule 1792, WSC emailed, paa, 8/26/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95412663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01400050","Sample-Routine","Water","Groundwater","2013-10-29","10:40:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-402504093364301",null,"A-3030141 VOC'S HAVE 3 DROPS HCL EACH VIAL  GW-RADCHEM--(6)- 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Box Alone)   Sampled @ 1240",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96766746","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300482","Sample-Routine","Water","Groundwater","2013-09-12","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303404091325402",null,"L-2560167 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96471666","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302623","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-293938095561301",null,"L-2190145 Sta ID corrected from 561400 to 561301 per Ging,paa,9/10/13  Missing fields mandatory for WHOI,paa Samples were received chilled at the WHOI lab.  X = Time not on RADON  Sta ID corrected from 561400 to 561301 per Ging,paa,9/10/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95466090","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300115","Sample-Routine","Water","Groundwater","2013-07-17","12:00:00","EDT",{"$nulls":4},490,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-360626083170401",null,"A-2000117 3 drops of HCL added to VOCs  Actual Radon Time: 1309 L-2000117 Received July 18, 2013..  S2437 split to 20132000305, paa, 3/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95443580","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300280","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394147119580801",null,"L-2380143 Received August 23,2013..  invalid med code GW corrected to WG, paa, 8/31/13  Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96429683","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300326","Sample-Routine","Water","Groundwater","2013-08-14","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-295446091403901",null,"L-2270150 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95516191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300789","Sample-Routine","Water","Groundwater","2013-08-19","11:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383056075500201",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95663386","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300911","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","CDT",{"$nulls":6},"Below land-surface datum",283,"feet",323,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334100088193001",null,"L-2420356 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96364177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306278","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","PDT",{"$nulls":4},96,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380204",null,"L-2340193 Received August 21, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96074450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400070","Sample-Routine","Water","Groundwater","2013-10-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335943085032801",null,"L-2970176 LC1369 deleted from this ASR, paa  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96755304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300276","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375224117145401",null,"L-2410074 Received August 28, 2013..  invalid med code GW corrected to WG, paa, 9/5/13  Received August 28, 2013  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96429232","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300944","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","EDT",{"$nulls":4},38,"feet",null,35,"feet",55,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-395259083561501",null,"L-2350169 Received August 22, 2013  Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96540973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300111","Sample-Routine","Water","Groundwater","2013-08-05","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311928085494201",null,"L-2180068 Samples were received chilled at the WHOI lab.","Tallahatta Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96823327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300224","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-15","09:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322025111033101",null,"L-1970157 S2437 split to 20131970172, paa, 3/13/14  Samples leaked a little cpm <20 7/16/13, TAL  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94987231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300979","Sample-Routine","Water","Groundwater","2013-08-27","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",53,"feet",83,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435200084280001",null,"L-2410118 Btl type is FUS, paa Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96406114","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300200","Sample-Routine","Water","Groundwater","2013-08-22","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350108089242401",null,"A-2380070 2 drops HCl added to VOCs L-2380070 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96510398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302194","Sample-Routine","Water","Groundwater","2013-09-23","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312235084095301",null,"L-2670020 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96631329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302183","Sample-Routine","Water","Groundwater","2013-08-29","18:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-314356084375901",null,"L-2420348 Received August 30, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96603610","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300058","Sample-Routine","Water","Groundwater","2013-06-25","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361802088194201",null,"A-1770042 H2S odor present     2 drops HCl in VOCs  H2S odor present     Actual sample collection time 1145 L-1770042 H2S odor present cmt added per Jim, paa, 6/26/13..  S2437 split to 20131770131, paa, 2/18/14  H2S odor present cmt added per Jim, paa, 6/26/13  Samples were received chilled at the W","McNairy Formation","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95009647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300140","Sample-Routine","Water","Groundwater","2013-08-20","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350253089323901",null,"L-2330060 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96423743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303373","Sample-Routine","Water","Groundwater","2013-07-23","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-461703088043901",null,"L-2060132 Received July 24, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113282579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305665","Sample-Routine","Water","Groundwater","2013-07-23","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364259119385402",null,"L-2060023 Received July 24, 2013..  GWMSA added to ASR for WSC,paa,8/2/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95324858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302626","Sample-Routine","Water","Groundwater","2013-08-21","10:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-431045095413901",null,"L-2350103 X = Sta id on sample 431118095401.  Updated station ID from 431118095413401 as per Shannon Stubbs, KMS11/07/2013  Samples were received chilled at the WHOI lab.  Updated station ID from 431118095413401 as per Shannon Stubbs, KMS11/07/2013  Updated SID from 431118095415401 per Stubbs.  KB 0",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96422865","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301069","Sample-Routine","Water","Groundwater","2013-08-29","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344323076451301",null,"L-2420331 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96378056","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300243","Sample-Routine","Water","Groundwater","2013-07-24","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305500091065201",null,"L-2070072 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95082355","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300150","Sample-Routine","Water","Groundwater","2013-07-31","12:00:00","EDT",{"$nulls":4},0,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351019084365501",null,"A-2130165 2 drops of HCL added to VOCs  Actual Radon time = 1325 L-2130165 Updated SID from 351002084372001 per Kingsbury.  KB 09/30/13  Samples were received chilled at the WHOI lab.  Updated SID from 351002084372001 per Kingsbury.  KB 09/30/13",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-96435297","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01400144","Sample-Routine","Water","Groundwater","2013-12-03","10:45:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384457091271701",null,"L-3390014 per Paul GWMSA added, pwg  Invalid NAWQA proposal corrected, paa Samples were received chilled at the WHOI lab.  X=1 GCV vial recvd empty    per Paul GWMSA added, pwg",null,"Not applicable","Not applicable",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-96973874","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300693","Sample-Routine","Water","Groundwater","2013-07-17","13:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-392359075370301",null,"L-2040030 Received July 19, 2013..  S2437 split to 20132040230, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94988152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301074","Sample-Routine","Water","Groundwater","2013-09-05","11:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345730078301702",null,"L-2490348 4436 vial 2 GCV not recvd, ASR time changed to match btls per Fitzgerald, paa, 9/6/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-11","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300118","Sample-Routine","Water","Groundwater","2013-08-21","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321505086104601",null,"L-2350054 Received August 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96911961","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302677","Sample-Routine","Water","Groundwater","2013-08-21","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303000095002001",null,"L-2350179 Received August 22, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = Date on sample 8/12/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95677221","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300163","Sample-Routine","Water","Groundwater","2013-09-11","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333924086352901",null,"L-2550119 verified HFL recvd, not indicated as shipped, paa, 9/24/13..  sta id changed to 333924086352701 per Gill, paa, 10/30/13  ASRs recvd late & entered 1/21/14, paa     corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab..  sta id changed to 333924086352","Fort Payne Chert/formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97173275","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300969","Sample-Routine","Water","Groundwater","2013-08-07","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345051078012103",null,"L-2240084 Received August 9, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95454344","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400243","Sample-Routine","Water","Groundwater","2013-11-20","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370200120280001",null,"L-3290106 X=a PEST is a PEST, not a GCV    Received November 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775206","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300788","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382439079344801",null,"L-2340310 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95670220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300708","Sample-Routine","Water","Groundwater","2013-07-24","12:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383231075383101",null,"L-2070134 Received July 25, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95056279","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300922","Sample-Routine","Water","Groundwater","2013-09-25","14:00:00","EDT",{"$nulls":4},259,"feet",null,575.5,"feet",796,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372148076461001",null,"L-2700161 Received September 26, 2013  ASR future smpl date of 20130928 corrected to match Radon as 20130925, paa, 9/30/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96616244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300108","Sample-Routine","Water","Groundwater","2013-08-06","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335103080230801",null,"L-2190076 Samples were received chilled at the WHOI lab.  Sch 1792, not LC, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95413151","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301856","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","EDT",{"$nulls":4},45,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310913084195301",null,"L-2190136 Updated time from 110000  per Buell.  KB 10/24/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95654715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302114","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-310552084435601",null,"L-2210148 Received August 08, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96549892","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305542","Sample-Routine","Water","Groundwater","2013-07-10","13:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365516120033401",null,"L-1930108 Received July 11, 2013..  S2437 split to 20131930245, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94887660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300090","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314647085333501",null,"L-2320155 Updated SID from 314658085331201 per Gill.  KB 4/11/14  One bottle did not list date & time per TALWA, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.     corrected station id per Gill   pwg  04/18/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96811163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303649","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452733089435101",null,"L-2550111 X = Time on DOC is 1201, the rest of the bottles have the correct time  ASRs recvd late & entered 1/21/14, paa  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113298638","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300832","Sample-Routine","Water","Groundwater","2013-08-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-374426079211101",null,"L-2400078 Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107025926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302915","Sample-Routine","Water","Groundwater","2013-09-09","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-260204097443701",null,"L-2530042 Updated STAID from 260212097444301 as per Patty 10.23.14 MKS.  ASRs recvd late & entered 1/21/14, paa. Updated STAID from 260212097444301 as per Patty 10.23.14 MKS.  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301260","Sample-Routine","Water","Groundwater","2013-09-24","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362244077015501",null,"L-2690096 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96580695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301389","Sample-Routine","Water","Groundwater","2013-09-16","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-440435091404901",null,"A-2600163 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6) - 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Exact Time: 1149  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2600163 Samples were received chilled at the W",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96491554","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300294","Sample-Routine","Water","Groundwater","2013-08-14","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312658109360401",null,"L-2270082 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95513823","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302651","Sample-Routine","Water","Groundwater","2013-09-16","10:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-412938092380601",null,"L-2610026 Received September 17, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96490482","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400291","Sample-Routine","Water","Groundwater","2013-12-03","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365100120060001",null,"L-3380013 X=a PEST is a PEST not a GCV. FA is not labeled with date/time and station id  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776092","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302966","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271843098401101",null,"L-2620041 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96495760","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300151","Sample-Routine","Water","Groundwater","2013-07-18","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310630085355601",null,"L-2000277 X = No station id on samples..  S2437 split to 20132000313, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = No station id on sample",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97057695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305888","Sample-Routine","Water","Groundwater","2013-08-14","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372505",null,"L-2270202 FA btl condition changed to improper preservation, JNV   Lab acidification lab code 3105 added, JNV    FA preserved by C.Harris on 8/19/13 @ 1005, JNV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95540441","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303021","Sample-Routine","Water","Groundwater","2013-09-24","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292923095091601",null,"L-2690194 Received September 25, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96555387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300612","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","CDT",{"$nulls":4},23,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444747096272001",null,"L-2700146 X = Improper sample container for DOC btl w/teal cap    Received September 26, 2013..   invalid NAWQA proposal corrected to CL13NAWSD to complete log in of custom requests and bill properly,paa,10/22/13  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab.  P",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96726466","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301328","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-400021077303101",null,"L-2540079 ASRs recvd late & entered 1/21/14, paa  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  FED EX LATE DELIVERY",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96409324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303382","Sample-Routine","Water","Groundwater","2013-08-01","14:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-454258088411601",null,"L-2140187 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113286444","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303433","Sample-Routine","Water","Groundwater","2013-08-05","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-433215088010001",null,"L-2190094 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113292256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400071","Sample-Routine","Water","Groundwater","2013-11-04","14:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380139077212901",null,"L-3090023 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96837255","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303647","Sample-Routine","Water","Groundwater","2013-09-09","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-442100089030001",null,"L-2530033 X = RU, FU, FCC & DOC have no time on sample  ASRs recvd late & entered 1/21/14, paa  Sta id on btl different from ASR per WHOI, sta id on btl 44210008930001, paa, 10/25/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113298176","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-11","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301226","Sample-Routine","Water","Groundwater","2013-09-17","15:45:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353143076575701",null,"L-2630119 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110390359","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301225","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351119076404801",null,"L-2630111 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110389902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300220","Sample-Routine","Water","Groundwater","2013-06-27","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-321321110450101",null,"L-1790118 S2437 split to 20131790271, paa, 2/18/14  Bottles have sample time @ 11:30, per TAL, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1130",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94867231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301403","Sample-Routine","Water","Groundwater","2013-09-24","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-454805096280901",null,"A-2690071 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM-- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH 2  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1311  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-2690071 Received September 25, 2013  Sample",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96552179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300687","Sample-Routine","Water","Groundwater","2013-07-16","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384152075290401",null,"L-1990092 Received July 17, 2013..  S2437 split to 20131990205, paa, 3/14/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104083149","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300198","Sample-Routine","Water","Groundwater","2013-08-15","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-334021079501308",null,"L-2310081 S1792 not LC1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95650087","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300050","Sample-Routine","Water","Groundwater","2013-06-26","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-342455080045509",null,"L-1780152 S2437 split to 20131780189, paa, 2/18/14  Invalid LC1792 corrected to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94849214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305612","Sample-Routine","Water","Groundwater","2013-07-25","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364457119553501",null,"L-2100109 S2437 PEST split to separate ASR @1331, paa, 7/29/13    Received July 26, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95227473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01400375","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-13","10:00:00","CST",{"$nulls":4},268,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-293516098325501",null,"L-3180136 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible helical rotor pump","NWIS-96944992","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301271","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-402058076124101",null,"L-2390146 Samples were received chilled at the WHOI lab.  sta id corrected from 40305 to 40205 per Low, paa, 1/3/14",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96051022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301230","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343855078315701",null,"L-2680058 Received September 24, 2013  Samples were received chilled at the WHOI lab.  X = recvd without ASR Eric faxed",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96504664","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302221","Sample-Routine","Water","Groundwater","2013-09-17","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323336084050601",null,"L-2610069 X = A PHARM is not a GCV  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96701634","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01301819","Sample-Routine","Water","Groundwater","2013-09-30","10:20:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-402332091342901",null,"L-2970126 Login delayed due to gov shutdown, ok to log recvd 10/24 from Paul B., paa, 10/24/13   Received October 01, 2013  File recvd late from TAL, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96604163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300082","Sample-Routine","Water","Groundwater","2013-07-15","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-313139085402101",null,"L-1990008 X = Samples do not have station id    Received July 16, 2013..  S2437 split to 20131990194, paa, 3/13/14  Samples were received chilled at the WHOI lab.  X = Station id not on label","Providence Sand","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96795508","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301395","Sample-Routine","Water","Groundwater","2013-09-18","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-435217095063401",null,"A-2620087 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6) - 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1155  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2620087 Samples were received chilled at the",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96492675","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300133","Sample-Routine","Water","Groundwater","2013-08-12","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-322405087342601",null,"L-2250122 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96912544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300324","Sample-Routine","Water","Groundwater","2013-08-27","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-353232114200501",null,"L-2400155 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96279525","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300919","Sample-Routine","Water","Groundwater","2013-09-26","10:00:00","EDT",{"$nulls":4},100,"feet",null,190,"feet",208,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372823076433601",null,"L-2950071 Login delayed due to gov shutdown, ok log per B.Lindsey, paa, 10/22/13    Received September 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible helical rotor pump","NWIS-96615768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300945","Sample-Routine","Water","Groundwater","2013-09-30","12:00:00","EDT",{"$nulls":4},315,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-381531076583001",null,"L-2950073 Login delayed due to gov shutdown,ok log per B. Lindsey,paa,10/22/13   Received October 1,2013  File recvd late from TAL, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96781492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302202","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321838084435101",null,"L-2660027 Received September 20, 2013  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96633103","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01400374","Sample-Routine","Water","Groundwater","2013-11-14","09:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292331098294501",null,"L-3220033 Received November 15, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-96944555","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300070","Sample-Routine","Water","Groundwater","2013-07-30","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322643087020001",null,"L-2130003 Updated SID from 322644087020201 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14","Coker Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96776124","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300431","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324858109510701",null,"L-2320058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97321453","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303450","Sample-Routine","Water","Surface Water","2013-05-20","12:15:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05451210",null,"L-1410060 Evn. ASR & smpls changed to 1215 per K.Romanok, paa, 5/21/13..  LC8252 deleted per Rose, paa, 5/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300913","Sample-Routine","Water","Groundwater","2013-08-28","14:30:00","CDT",{"$nulls":6},"Below land-surface datum",2210,"feet",2280,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332240089033401",null,"L-2410237 Samples were received chilled at the WHOI lab.  X = Time on samples 1430..  time added to ASR per radon, paa, 9/5/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96364801","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01303486","Sample-Routine","Water","Groundwater","2013-07-31","11:40:00","MDT",{"$nulls":4},5.8,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-402213104015501",null,"A-2140132 6 drops HCl each for schedules 4436 and 4437.","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95387948","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301149","Sample-Routine","Water","Groundwater","2013-09-10","10:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341758077480802",null,"L-2550063 X = No time on RU  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443932","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306349","Sample-Routine","Water","Groundwater","2013-08-27","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364400119450001",null,"L-2470093 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96371045","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303418","Sample-Routine","Water","Groundwater","2013-08-07","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444302089144401",null,"L-2210439 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113290029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301223","Sample-Routine","Water","Groundwater","2013-09-17","08:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350717077002001",null,"L-2630113 X = Date on samples 9-17-13  Updated date from 2013/09/13 per Pointer.  KB 12/16/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110388985","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306358","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363500120030001",null,"L-2410019 Received August 28, 2013  Samples were received chilled at the WHOI lab.  smdugan added, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96371910","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300174","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","CDT",{"$nulls":4},98,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350543089473901",null,"A-2270007 3 drops HCl added to VOCs L-2270007 Received August 14, 2013  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96464256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301348","Sample-Routine","Water","Groundwater","2013-09-12","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-463618094183101",null,"A-2560042 VOCs HAVE 5 DROPS HCL EACH VIAL   Pleas lab filter schedule 2434  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH 2   LC=1364, LC=2164, shipped in 2nd cooler  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Actual time = 1335  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96448793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303374","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-460308088130601",null,"L-2110172 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300582","Sample-Routine","Water","Groundwater","2013-06-05","11:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385009075444401",null,"L-1580144 Received June 6, 2013,  STA ID corrected to 385009075444401 per Bringman GB 9/3/13..  S2437 split to 20131580152, paa, 2/14/14  STA ID corrected to 385009075444401 per Bringman GB 9/3/13",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94559591","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303377","Sample-Routine","Water","Groundwater","2013-07-30","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-451854087545501",null,"L-2130206 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113284297","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306281","Sample-Routine","Water","Groundwater","2013-08-20","09:00:00","PDT",{"$nulls":4},148,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380203",null,"L-2340191 Received August 21, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96159326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400078","Sample-Routine","Water","Groundwater","2013-10-24","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345255085174201",null,"L-3010111 Received October 25, 2013..  LC1369 removed from this ASR, paa, 11/4/13  Btl type FUS, not GCC, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96763067","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300404","Sample-Routine","Water","Groundwater","2013-08-21","12:00:00","MST",{"$nulls":4},75,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325104109421001",null,"L-2350253 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96935655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400457","Sample-Routine","Water","Groundwater","2013-12-09","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700119470002",null,"L-3450047 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776976","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302563","Sample-Routine","Water","Groundwater","2013-08-13","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-421016092020201",null,"L-2260157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95679968","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305541","Sample-Routine","Water","Groundwater","2013-07-11","10:10:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365418120035101",null,"L-1970165 S2437 split to 20131970173, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94887240","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301224","Sample-Routine","Water","Groundwater","2013-09-17","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350513076501501",null,"L-2630121 One btl recvd without label per Testam, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110389445","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301269","Sample-Routine","Water","Groundwater","2013-09-24","16:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351731076514101",null,"L-2700088 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110393177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301685","Sample-Routine","Water","Groundwater","2013-08-19","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414400112050001",null,"L-2330051 ASR missing med code and smpl type, WG/9 added per PEST ASR, paa, 8/29/13  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-95681871","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01302838","Sample-Routine","Water","Groundwater","2013-09-18","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-393922096114901",null,"L-2630162 X = 1 GCV has date 9/?/2013  Btl type for Sch2255 i FUS, paa Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97186914","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301207","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":4},17,"feet",null,20,"feet",28,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-411432088234001",null,"L-2390164 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95912157","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301861","Sample-Routine","Water","Groundwater","2013-08-08","12:30:00","EDT",{"$nulls":4},22,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-311015084511901",null,"A-2210433 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-95668982","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300052","Sample-Routine","Water","Groundwater","2013-07-10","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354601084084201",null,"A-1930090 3 drops HCL added to VOC's  Actual Sample Time = 13:03 L-1930090 Received July 11, 2013   X = Please do not use pencil on ASR..  S2437 split to 20131930241, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94977484","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300286","Sample-Routine","Water","Groundwater","2013-09-04","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393351116000101",null,"L-2490177 Corrected med code to WG, paa   Recvd 9/6/13  Recvd 9/6/13  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96467946","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400242","Sample-Routine","Water","Groundwater","2013-11-19","10:20:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370800120270001",null,"L-3240015 X=PEST is PEST not GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300433","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310305092101202",null,"L-2400177 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96360558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300064","Sample-Routine","Water","Groundwater","2013-07-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-332036079244009",null,"L-2000084 Received July 18, 2013..  S2437 split to 20132000304, paa, 3/14/14  Corrected LC1792 to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94954827","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400459","Sample-Routine","Water","Groundwater","2013-12-10","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370200119590001",null,"L-3450049 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300169","Sample-Routine","Water","Groundwater","2013-08-14","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335323088074301",null,"L-2270136 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97177368","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WV","USGS West Virginia Water Science Center","nwiswv.01.01300172","Sample-Routine","Water","Groundwater","2013-08-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392158077525301",null,"L-2320020 X = Samples have date 8-19-13   Begin date is missing in mandatory field, time = 1100, JNV..  date added to ASR per btls, paa, 8/26/13..  User Code VA changed to WV per A. Melberg, paa, 9/10/13  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  User Code VA changed to WV",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96337224","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306534","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420001",null,"L-2610074 Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96538536","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301628","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401012111354801",null,"L-2270198 Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95475574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300238","Sample-Routine","Water","Groundwater","2013-07-23","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302602091002505",null,"L-2060069 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95081886","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303022","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-291949095024801",null,"L-2690191 Received September 25, 2013  Updated SID from 292037095010501 per Ging.  KB 8/5/14  FUS btl type, paa Samples were received chilled at the WHOI lab.  Received September 25, 2013   Updated SID from 292037095010501 per Ging.  KB 8/5/14  Updated SID from 292037095010501 per Ging.  KB 8/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921974","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305563","Sample-Routine","Water","Groundwater","2013-07-09","08:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-333700114340001",null,"L-1910081 S2437 split to 20131910107, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96048698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302169","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320051084061401",null,"A-2270163 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96562950","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301263","Sample-Routine","Water","Groundwater","2013-09-25","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355840076571001",null,"L-2730028 Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96582061","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300942","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",177,"feet",197,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-403857082191101",null,"L-2270191 Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96559910","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303632","Sample-Routine","Water","Groundwater","2013-08-21","17:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-442008089135201",null,"L-2380161 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113294745","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400072","Sample-Routine","Water","Groundwater","2013-10-23","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-341529085071301",null,"L-2970178 LC1369 deleted from this ASR, paa  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96754845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300115","Sample-Routine","Water","Groundwater","2013-09-11","08:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333642086065001",null,"L-2550121 X  =Time on samples 0900..  verified HFL recvd, not indicated as shipped, paa, 9/12/13   Updated SID from 333642086065101 per Gill.  KB 4/11/14  ASRs recvd late & entered 1/21/14, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.     corre",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96888911","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303415","Sample-Routine","Water","Groundwater","2013-08-08","15:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435453089184701",null,"L-2210437 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113289584","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300114","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-315522087045901",null,"L-2330058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96889501","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300316","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354709115220001",null,"L-2680157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96730762","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300326","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-353513114161701",null,"L-2410259 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96280146","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300336","Sample-Routine","Water","Groundwater","2013-09-04","09:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320138111165301",null,"L-2480050 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96400549","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300330","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345516114364901",null,"L-2420145 FED EX LATE DELIVERY  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96278913","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305216","Sample-Routine","Water","Groundwater","2013-06-10","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-372100118250001",null,"L-1620245 S2437 split to 20131620256, paa, 2/14/14  GWMSA added due to exception, paa, 6/13/13  Samples were received chilled at the WHOI lab.  D-R'd per Mullin, sample ruined at contract lab.  KB 10/29/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94737897","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305596","Sample-Routine","Water","Groundwater","2013-07-15","10:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-345006118125701",null,"L-1990052 Received July 16, 2013..  S2437 split to 20131990197, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95016292","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303376","Sample-Routine","Water","Groundwater","2013-07-25","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452121088541301",null,"L-2110168 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01400007","Sample-Routine","Water","Groundwater","2013-11-06","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375700114254801",null,"L-3110028 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96891758","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300910","Sample-Routine","Water","Groundwater","2013-09-23","14:00:00","EDT",{"$nulls":6},"Below land-surface datum",279,"feet",354,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-374550077300501",null,"L-2680054 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96614340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302212","Sample-Routine","Water","Groundwater","2013-09-17","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323316084140501",null,"L-2610067 X = PHARM is not a GCV  Btl type is FUS, ASR missing mandatory pH, paa, 10/28/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96701171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301404","Sample-Routine","Water","Groundwater","2013-09-26","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-454900094342101",null,"L-2730066 Received September 27, 2013  Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96552765","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303656","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-432700089440001",null,"L-2350223 X = Date on samples 8/21/2013   Updated date from 2013/08/22 per Manteufel.  KB 02/03/14  Samples were received chilled at the WHOI lab.  radon recvd without smpl info on cylinder or smpl, added label per ASR, WSC emailed, paa, 8/22/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113299165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301258","Sample-Routine","Water","Groundwater","2013-09-23","14:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354953076484101",null,"L-2690100 X = GCV vial recvd broken  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96579784","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301266","Sample-Routine","Water","Groundwater","2013-09-23","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352301077300701",null,"L-2700086 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110391808","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300955","Sample-Routine","Water","Groundwater","2013-07-09","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352832076470102",null,"L-1920048 RECEIVED JULY 10, 2013..  S2437 split to 20131920163, paa, 2/19/14    X = Please correct your btl labels for SCH 2437, pest & LC 9017 Pharm.  They are not GCV's   LC's not indicated as add or delete, LC's added.  CSH  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-103032770","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301790","Sample-Routine","Water","Groundwater","2013-09-11","08:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394200111490001",null,"L-2550014 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96440191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300741","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","CDT",{"$nulls":6},"Below land-surface datum",832,"feet",863,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342409088520901",null,"L-2100009 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95379365","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305616","Sample-Routine","Water","Groundwater","2013-07-22","14:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363806119345301",null,"L-2050201 Received July 23, 2013..  S2437 split to 20132050229, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95229190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301148","Sample-Routine","Water","Groundwater","2013-09-09","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343726078360201",null,"L-2550065 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443472","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301154","Sample-Routine","Water","Groundwater","2013-09-12","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352839077040701",null,"L-2560053 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110388041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300735","Sample-Routine","Water","Groundwater","2013-07-24","15:45:00","CDT",{"$nulls":6},"Below land-surface datum",1609,"feet",1689,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345216089400201",null,"L-2100003 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95378132","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306533","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-17","09:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420002",null,"L-2610076 Samples were received chilled at the WHOI lab..  Sta ID changed to 364200119420002 per Dugan, paa, 3/21/14",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96538091","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300281","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-385738119433601",null,"L-2320053 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96428784","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300161","Sample-Routine","Water","Groundwater","2013-07-16","11:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312534085203401",null,"L-1990082 X = No station id on samples    Received July 17, 2013..  S2437 split to 20131990199, paa, 3/13/14  Updated SID from 312517085201801 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.     corrected station id per Gill   pwg  04/18/14  X = You need to put station id on yo",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97172773","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300285","Sample-Routine","Water","Groundwater","2013-09-03","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392933117061701",null,"L-2470086 invalid med code GW corrected to WG, WSC notified, paa, 9/7/13  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96467494","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300676","Sample-Routine","Water","Groundwater","2013-06-25","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",315,"feet",345,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311642090113601",null,"L-1780043 Received June 26, 2013..  S2437 split to 20131780187, paa, 2/18/14  Received June 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94780770","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301071","Sample-Routine","Water","Groundwater","2013-09-03","16:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344734077254601",null,"L-2490159 Radon recvd completely unlabeled, added label per ASR, WSC notified requesting verify, paa, 9/4/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96378578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300717","Sample-Routine","Water","Groundwater","2013-07-30","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-393254075531801",null,"L-2130017 Received July 31, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95321788","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305213","Sample-Routine","Water","Groundwater","2013-06-11","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-342953117173101",null,"L-1630037 S2437 split to 20131630117, paa, 2/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94738454","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300137","Sample-Routine","Water","Groundwater","2013-09-16","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-334821086090001",null,"L-2610031 X = Improper sample container for RU in 1L glass bottle  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96918391","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300292","Sample-Routine","Water","Groundwater","2013-08-15","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-314322110030901",null,"L-2280189 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95513204","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300118","Sample-Routine","Water","Groundwater","2013-07-18","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355047084082701",null,"A-2030048 Drops of HCl added to VOCs  Actual Radon Time: 1212 L-2030048 Received July 19, 2013..  S2437 split to 20132030166, paa, 3/17/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95444192","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300170","Sample-Routine","Water","Groundwater","2013-08-20","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350403089445201",null,"L-2330062 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96463385","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300894","Sample-Routine","Water","Groundwater","2013-09-16","11:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393241077434201",null,"L-2600149 Updated UC from PA per Dieter.  KB 11/18/13  2 caps broken, sample for alpha beta empty, per testam, paa  Updated UC from PA per Dieter.  KB 11/18/13  Samples were received chilled at the WHOI lab.  Updated UC from PA per Dieter.  KB 11/18/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Other","NWIS-96479376","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300141","Sample-Routine","Water","Groundwater","2013-05-01","14:45:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392927119475201",null,"L-1230039 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131230103, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94382991","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300674","Sample-Routine","Water","Groundwater","2013-06-19","11:15:00","CDT",{"$nulls":6},"Below land-surface datum",210,"feet",250,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315920089541701",null,"L-1710186 S2437 split to 20131710195, paa, 2/18/14  1369 is lab code, not schedule, paa  Chg'd to S1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94772526","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301167","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","CDT",{"$nulls":6},"Below land-surface datum",18,"feet",28,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393232088221801",null,"L-2320066 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95545324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305682","Sample-Routine","Water","Groundwater","2013-07-30","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364639120065001",null,"L-2130124 S2437 deleted from this ASR, see 2nd ASR @1331 for PEST, paa, 8/10/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95371649","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300704","Sample-Routine","Water","Groundwater","2013-07-23","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-374755075371001",null,"L-2060179 Received July 24, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95055836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300425","Sample-Routine","Water","Groundwater","2013-09-05","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324937113304501",null,"L-2490270 X = Time on samples 1100  Samples were received chilled at the WHOI lab.  X = Time on sample 1100",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97320825","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300208","Sample-Routine","Water","Groundwater","2013-08-14","14:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350018089190701",null,"A-2270187 2 drops HCl added to VOCs L-2270187 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96511276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300206","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350625089554901",null,"A-2410042 2 drops HCl/VOC vial L-2410042 Received August 28, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96509517","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300145","Sample-Routine","Water","Groundwater","2013-04-29","11:15:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391126119423201",null,"L-1210155 Lab codes not indicated as add or delete, LC's added, JNV..  one GCV converted to PEST and added, prog code corrected to GWMSA WSC notified, paa, 5/2/13..  S2437 split to 20131210174, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94425121","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300204","Sample-Routine","Water","Groundwater","2013-09-11","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351231089392301",null,"A-2550041 2  drops HCl/VOC vial L-2550041 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96510832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303023","Sample-Routine","Water","Groundwater","2013-09-23","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300932094005301",null,"L-2680148 Received September 24, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96555820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306553","Sample-Routine","Water","Groundwater","2013-09-24","11:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364100119440001",null,"L-2680178 Smpl type changed from 1 to 9 per Evans, paa, 9/25/13     DOC condition changed to improper preservation, JNV  Samples were received chilled at the WHOI lab.  WSC emailed regarding smpl type 1, paa   Changed smpl type to 9 per Dugan, paa, 10/31/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96576242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305617","Sample-Routine","Water","Groundwater","2013-07-23","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363928119401701",null,"L-2070165 X = Station ID diff. on btls's 363928119401701  PEST split to separate ASR @ 1001, paa 7/26/13  Received July 25, 2013,  STAID changed to 363928119401701 per Bennett GB 9/3/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95232156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300785","Sample-Routine","Water","Groundwater","2013-08-15","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385634078261501",null,"L-2280112 Btl type is FUS, paa   Begin date is missing in mandatory field, time = 1100, JNV Samples were received chilled at the WHOI lab.  date added to ASR per NWQL ASR, paa, 9/7/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107025473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302965","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271505098073401",null,"L-2660071 Received September 20, 2013  Updated SID per Ging. 8/5/14  FUS btl type,paa Samples were received chilled at the WHOI lab.  Sta ID changed to 271505098073401 per Ging, paa, 9/25/14  Updated SID per Ging. 8/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921542","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306284","Sample-Routine","Water","Groundwater","2013-08-19","14:40:00","PDT",{"$nulls":4},105,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380202",null,"L-2380206 ASR sta id corrected to match btls & per Dugan and fields corrected too, paa, 8/26/13  Updated SID from 364258119380201 per Dugan.  KB 09/10/13  Lid was off of one bottle (alpha/beta) and entire volume was lost   Station id on bottle is: 364258119380202   ASR sta id corrected per Dugan",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96074884","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300221","Sample-Routine","Water","Groundwater","2013-07-10","11:15:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333051112082001",null,"L-1930036 Received Jul 11, 2013..  S2437 split to 20131930238, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94924871","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303378","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-30","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-454107088011001",null,"L-2130208 S2437 deleted from this ASR, see second @1331, paa, 8/10/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113284726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300348","Sample-Routine","Water","Groundwater","2013-08-19","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313610091504501",null,"L-2320151 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95555138","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300277","Sample-Routine","Water","Groundwater","2013-07-30","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-344152111592301",null,"L-2130032 Received July 31, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95389988","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302554","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-430449096061301",null,"L-2380244 logged from problem cooler, paa  Samples were received chilled at the WHOI lab.  logged from problem cooler, smpl information added to GCVs by paa, 8/26/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95678562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300088","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314038085365401",null,"L-2390168 X = Time on sample 1200",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96801601","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01301526","Sample-Routine","Water","Surface Water","2013-05-13","11:40:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-324305097101900",null,"L-1350041 Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300666","Sample-Routine","Water","Groundwater","2013-07-08","14:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-373330075494601",null,"L-1920036 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131920161, paa, 2/19/14",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94892623","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300167","Sample-Routine","Water","Groundwater","2013-07-24","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-321100086344501",null,"L-2070098 Received July 25, 2013..  PEST and S2437 split to second ASR @1130, Lab ID 20132070161, paa, 7/26/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97176757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300696","Sample-Routine","Water","Groundwater","2013-07-18","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385715075253001",null,"L-2030146 Received July 19, 2013..  S2437 split to 20132030167, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-94988597","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300331","Sample-Routine","Water","Groundwater","2013-08-15","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-312038092192601",null,"L-2280129 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95515726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306344","Sample-Routine","Water","Groundwater","2013-08-28","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364100119450001",null,"L-2420373 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96373509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300053","Sample-Routine","Water","Groundwater","2013-07-15","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353857084511801",null,"A-1990033 3 drops HCl added to VOCs  Actual Radon Sample Time: 14:13 L-1990033 Received July 16, 2013..  S2437 split to 20131990196, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94978083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301372","Sample-Routine","Water","Surface Water","2013-03-12","15:20:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02281200",null,"L-0730004 Updated time from 1500 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107230079","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-03-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302859","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-280951096593801",null,"L-2410129 FUS btl type, paa Samples were received chilled at the WHOI lab.  Lid was completely off one sample, but lost small amount of sample (aprox 150-175mLs) per Test Am, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368442","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PR","USGS Puerto Rico Water Science Center","nwispr.01.01301107","Sample-Routine","Water","Surface Water","2013-03-19","10:40:00","AST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-50055410",null,"L-0790103 Updated time from 103000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107219605","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-03","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302621","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292944095550101",null,"L-2210241 Received August 08, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = Time of sample label 1006",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95465216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300086","Sample-Routine","Water","Groundwater","2013-07-08","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323528086205801",null,"L-1900068 S2437 split to 20131900099, paa, 2/19/14  Samples were received chilled at the WHOI lab.  X = Please put information on tube so that we do not have to open, PG","Coker Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96800988","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300297","Sample-Routine","Water","Groundwater","2013-09-10","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-404325116065801",null,"L-2540077 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300100","Sample-Routine","Water","Groundwater","2013-08-08","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355752082564201",null,"A-2210431 3 drops of HCL added to VOCs  Actual Radon time =  1334 L-2210431 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95426613","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300736","Sample-Routine","Water","Groundwater","2013-07-24","12:45:00","CDT",{"$nulls":6},"Below land-surface datum",492,"feet",552,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343706089111601",null,"L-2100006 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95378734","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302619","Sample-Routine","Water","Surface Water","2013-04-16","10:10:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02335870",null,"L-1080111 Received April 17, 2013  Updated time from 100000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107221194","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300599","Sample-Routine","Water","Groundwater","2013-06-12","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390126075575401",null,"L-1640024 S2437 split to 20131640198, paa, 2/14/14",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94621681","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305207","Sample-Routine","Water","Groundwater","2013-06-13","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-335700116300001",null,"L-1690057 X = 9017 PHARM & 2434 HFL are not GCV's    Received June 14, 2013..  S2437 split to 20131690165, paa, 2/18/14  Samples were received chilled at the WHOI lab.  Updated SID from 33570011630001 per Dugan.  KB 07/11/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95906708","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300153","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-16","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354041084243601",null,"A-1990083 3 drops of HCL added to VOCs  Radon actual time = 1244 L-1990083 X = Please do not use pencil on ASR   Received July 17, 2013  Samples were received chilled at the WHOI lab.  corrected eASR sta id for Creekside per G. Johnson,paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96436487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302165","Sample-Routine","Water","Groundwater","2013-08-13","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312346084520401",null,"L-2270074 Received August 14, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96562393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400295","Sample-Routine","Water","Groundwater","2013-12-05","09:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370000120120001",null,"L-3400054 station id corrected per Sue D.  pwg 1/02/14  Samples were received chilled at the WHOI lab.   corrected station id per Sue D.  pg  5/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776798","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300202","Sample-Routine","Water","Groundwater","2013-09-12","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350327089421401",null,"A-2560154 2 drops HCl/VOC vial L-2560154 only 5 GCV vials recvd per Murtaugh, paa  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96509069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300668","Sample-Routine","Water","Groundwater","2013-07-10","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-380403075292901",null,"L-1960088 Received July 12, 2013..  S2437 split to 20131960102, paa, 2/20/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94893474","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300148","Sample-Routine","Water","Groundwater","2013-08-14","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350234089394504",null,"A-2270189 2 drops HCl added to VOCs L-2270189 Updated SID from 350235089394701 per Kingsbury.  KB 09/30/13  Samples were received chilled at the WHOI lab.  Updated SID from 350235089394701 per Kingsbury.  KB 09/30/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96425510","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302862","Sample-Routine","Water","Groundwater","2013-08-21","16:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301420095093201",null,"L-2350194 Received August 22, 2013    Per Ging changed station id from 301419095093301   pwg  2013/09/07  FUS btl type, paa Samples were received chilled at the WHOI lab.  Received August 22, 2013. Updated STAID from 301419095093301 as per Patty 10.23.14 MKS.  Updated STAID from 301419095093301 as p",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96369313","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301624","Sample-Routine","Water","Groundwater","2013-08-15","12:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401148112433002",null,"L-2310079 Samples were received chilled at the WHOI lab.","Valley Fill","Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible piston pump","NWIS-95475102","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300193","Sample-Routine","Water","Groundwater","2013-05-08","11:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391111119481901",null,"L-1340062 Received May 11, 2013..  S2437 split to 20131340161, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4060,"USGS parameter code 82398","Gas reciprocating pump",null,"Gas reciprocating pump","NWIS-94586331","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300270","Sample-Routine","Water","Groundwater","2013-08-06","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304612089512401",null,"L-2200021 Received August 7, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95430262","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300314","Sample-Routine","Water","Groundwater","2013-09-19","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405517114204101",null,"L-2630098 DOC condition changed to improper preservation, JNV  sta id correction per K. Thomas,paa,11/4/13  Samples were received chilled at the WHOI lab.  sta id correction per K. Thomas,paa,11/4/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96602216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01400009","Sample-Routine","Water","Groundwater","2013-11-07","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361200115580001",null,"L-3120076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96939011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300198","Sample-Routine","Water","Groundwater","2013-09-10","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351528089350801",null,"A-2540036 2 drops HCl added to VOCs L-2540036 ASRs recvd late & entered 1/21/14, paa..  Sta ID changed to 351528089350801 per Kingsbury, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96509954","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303381","Sample-Routine","Water","Groundwater","2013-08-01","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-462416088191901",null,"L-2140189 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113286014","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305585","Sample-Routine","Water","Groundwater","2013-07-17","10:50:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363107119372201",null,"L-2000067 Received July 18, 2013..  S2437 split to 20132000302, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985015","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301228","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-18","12:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354552077382301",null,"L-2630064 Samples were received chilled at the WHOI lab.  corrected station id per WSC  pwg  1/30/814  smpl type 9 corrected to 7 per Erik, paa, 10/31/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96503748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300792","Sample-Routine","Water","Groundwater","2013-08-21","09:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384322075394401",null,"L-2350145 Received August 22, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104233803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301152","Sample-Routine","Water","Groundwater","2013-09-11","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343908078432003",null,"L-2550059 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96445309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302855","Sample-Routine","Water","Groundwater","2013-09-05","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310935093352701",null,"L-2490137 FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96367572","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300428","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-314050091260501",null,"L-2380072 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96360106","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300985","Sample-Routine","Water","Groundwater","2013-08-29","09:00:00","EDT",{"$nulls":6},"Below land-surface datum",92,"feet",112,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-423200084490001",null,"L-2420479 Received August 31, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96407397","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301231","Sample-Routine","Water","Groundwater","2013-09-19","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342728077335701",null,"L-2680056 Received September 24, 2013  Samples were received chilled at the WHOI lab.  Updated SID from 342650077351501 per Pointer.  KB 01/10/14  X = Recvd without ASR Erik faxed corrected btl label per Brian, PG",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96505120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302620","Sample-Routine","Water","Groundwater","2013-08-08","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-290028095594700",null,"L-2210360 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = 1 FA recvd  X = Time on sample 1032",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95464775","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300298","Sample-Routine","Water","Groundwater","2013-09-11","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405030115500001",null,"L-2550083 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573942","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300300","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312423110574901",null,"L-2190150 Updated SID from 312443110573001 per Beisner.  KB 01/02/14  Dropped and cracked lids on 2 bottles during receipt. Lost small amount of volume. Transferred to new containers per TALWA      Updated SID from 312443110573001 per Beisner.  KB 01/02/14  Samples were received chilled at the WHOI",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95530757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305259","Sample-Routine","Water","Groundwater","2013-06-25","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-333130114394001",null,"L-1770062 DOC changed to improper preservation, paa..  GWMSA added, WSC to verify, paa, 6/29/13..  S2437 split to 20131770132, paa, 2/18/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125523816","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300149","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342640088065901",null,"L-1980064 X = No station id on samples..  S2437 split to 20131980174, paa, 3/13/14  Samples were received chilled at the WHOI lab.  X=Station ID not on label",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97057093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300723","Sample-Routine","Water","Groundwater","2013-07-11","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",1989,"feet",2074,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333618089074301",null,"L-1960028 Received Jul 12, 2013..  S2437 split to 20131960100, paa, 2/20/14  Received Jul 12,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95237689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305540","Sample-Routine","Water","Groundwater","2013-07-11","12:50:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365220120052601",null,"L-1970151 S2437 split to 20131970169, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94886821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301068","Sample-Routine","Water","Groundwater","2013-08-28","11:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344244077135801",null,"L-2420333 X = Only 2 GCVs for 4436 recvd  Few samples had loose lids and leaked. COCs were not in plastic bag and got soaked per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96377603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01400231","Sample-Routine","Water","Groundwater","2013-12-11","10:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302329087040001",null,"L-3460042 FUS btl typpe for S2255, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97164340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301073","Sample-Routine","Water","Groundwater","2013-09-04","14:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351804077520101",null,"L-2490155 ASR missing mandatory pH & alk, paa Samples were received chilled at the WHOI lab.  Per Shanon F.  corrected station id.  pwg  1/13/2014",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300721","Sample-Routine","Water","Groundwater","2013-07-09","10:45:00","CDT",{"$nulls":6},"Below land-surface datum",1480,"feet",1546,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325846088340801",null,"L-1910088 S2437 split to 20131910109, paa, 2/19/14  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95236492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300988","Sample-Routine","Water","Groundwater","2013-09-03","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",93,"feet",113,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-424900083150001",null,"L-2480071 Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96408037","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300976","Sample-Routine","Water","Groundwater","2013-08-26","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",150,"feet",185.8,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435000084510001",null,"L-2410124 Lab Codes not indicated as add or delete,lab codes added,AAN  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Samples received 8/29/13 @ 1015 am, 45 minutes left to run 2hr alpha beta per Test Am, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96405475","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305897","Sample-Routine","Water","Groundwater","2013-08-13","13:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372501",null,"L-2260083 Corrected to GWMSA, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95531694","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300746","Sample-Routine","Water","Groundwater","2013-07-23","12:30:00","CDT",{"$nulls":6},"Below land-surface datum",1303,"feet",1383,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341359089062201",null,"L-2060081 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95380599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400289","Sample-Routine","Water","Groundwater","2013-12-02","09:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365400120070001",null,"L-3380015 X=a PEST is a PEST, not a GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775737","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300135","Sample-Routine","Water","Groundwater","2013-08-15","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-332357087524301",null,"L-2280114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96913142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300219","Sample-Routine","Water","Groundwater","2013-07-01","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-325329112405301",null,"L-1840085 Received July 2,2013..  S2437 split to 20131840130, paa, 2/19/14  Released Gross alpha beta per Mullin.  KB 6/17/15  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94866626","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300916","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","EDT",{"$nulls":4},210,"feet",null,247,"feet",272,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372148076461002",null,"L-2700159 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96615293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300142","Sample-Routine","Water","Groundwater","2013-08-27","18:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350514089553700",null,"A-2410044 3 drops of HCl added to VOCs L-2410044 Received August 28, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96424178","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400018","Sample-Routine","Water","Groundwater","2013-10-28","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",477,"feet",538,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375541076514301",null,"L-3030063 Received October 29, 2013  Samples were received chilled at the WHOI lab.  sta id corrected to 4301 per A. Melberg, paa, 1/21/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96781964","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NE","USGS Nebraska Water Science Center","nwisne.01.01300271","Sample-Routine","Water","Surface Water","2013-06-10","10:10:00","CDT",{"$nulls":14},"USGS-06770195",null,"L-1640193 Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302645","Sample-Routine","Water","Groundwater","2013-09-18","10:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-415613094591201",null,"L-2620166 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96489562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301072","Sample-Routine","Water","Groundwater","2013-09-04","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344002077013201",null,"L-2490161 Samples were received chilled at the WHOI lab.  X = Date on sample 9/4/13..  ASR date corrected to match Radon, paa, 9/7/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300223","Sample-Routine","Water","Groundwater","2013-07-18","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-330135111231701",null,"L-2000244 S2437 split to 20132000307, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = Time on sample 1110",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-97152093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305593","Sample-Routine","Water","Groundwater","2013-07-16","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-344400117200001",null,"L-1990012 Received July 17, 2013..  S2437 split to 20131990195, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95016762","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301270","Sample-Routine","Water","Groundwater","2013-09-26","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354245077311701",null,"L-2730032 Received September 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110393632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306539","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364300119420001",null,"L-2610095 Missing alk, WSC emailed, 10/31/13, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400240","Sample-Routine","Water","Groundwater","2013-11-18","10:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370500120190001",null,"L-3240012 X=PEST is not GCV it is a PEST  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106774675","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305543","Sample-Routine","Water","Groundwater","2013-07-10","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365700120063401",null,"L-1930105 Received July 11, 2013    Btl type for S2437 is PEST,  paa..  S2437 split to 20131930242, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94888080","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300155","Sample-Routine","Water","Groundwater","2013-08-07","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-315820087202001",null,"L-2210136 Updated SID from 315915087202301 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97167396","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300879","Sample-Routine","Water","Groundwater","2013-09-19","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",618,"feet",659,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-373759076345501",null,"L-2660019 Received September 20, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96502818","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302200","Sample-Routine","Water","Groundwater","2013-09-18","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320859085003701",null,"L-2620156 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96632654","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400076","Sample-Routine","Water","Groundwater","2013-10-29","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344855084461101",null,"L-3030172 LC1369 removed from this ASR, paa, 11/4/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96762615","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400074","Sample-Routine","Water","Groundwater","2013-11-05","10:00:00","EST",{"$nulls":4},307,"feet",null,850,"feet",985,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365751076363001",null,"L-3100037 Date on btls 11/5/13..  corrected ASR date to match per A. Melberg, paa, 1/21/14  WSC emailed to verify field alk, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab...  field alk updated to 419.5 per Teunis, WHOI updated, paa, 11/13/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96837725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400027","Sample-Routine","Water","Groundwater","2013-10-31","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",215,"feet",316,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372105077113601",null,"L-3080057 Received November 1, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96783378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300066","Sample-Routine","Water","Groundwater","2013-07-10","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320848080454301",null,"L-1920128 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131920167, paa, 2/19/14  1792 is schedule, not lab code, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94955751","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","improper preservationsample was dilutedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300613","Sample-Routine","Water","Groundwater","2013-09-24","10:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-445330097071801",null,"L-2700147 X= Improper sample container for DOC btl w/teal cap    Received September 26, 2013..   invalid NAWQA proposal corrected to CL13NAWSD to complete log in of custom requests and bill properly,paa,10/22/13  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab. Sam",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96727024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301171","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-21","11:00:00","CDT",{"$nulls":4},60,"feet",null,77,"feet",102,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-383932090012601",null,"L-2350123 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95555768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300275","Sample-Routine","Water","Groundwater","2013-07-29","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-342557112041303",null,"L-2120035 PEST & Sch2437 split to second ASR, paa, 7/31/13   Time not on PHARM, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95389378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302198","Sample-Routine","Water","Groundwater","2013-09-24","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320348084132701",null,"L-2680108 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96632220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300265","Sample-Routine","Water","Groundwater","2013-07-31","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301407092104201",null,"L-2130178 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Grab sample","NWIS-95420211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300068","Sample-Routine","Water","Groundwater","2013-07-16","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333850079014308",null,"L-1990137 Received July 17, 2013     GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131990208, paa, 3/14/14  LC1792 corrected to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94990374","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300296","Sample-Routine","Water","Groundwater","2013-07-16","09:45:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315010111000701",null,"L-1990053 Received July 17, 2013..  S2437 split to 20131990198, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-95529513","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302914","Sample-Routine","Water","Groundwater","2013-09-10","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271315097473201",null,"L-2540057 1 cap broken, 3/4 sample missing per TAL   ASRs recvd late & entered 1/21/14, paa  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96454122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306555","Sample-Routine","Water","Groundwater","2013-09-25","13:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364306119364401",null,"L-2700140 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96575802","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303639","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-460000088235501",null,"L-2400181 Bottles have station id of 460000088265501, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113295868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400074","Sample-Routine","Water","Groundwater","2013-10-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-343914085165901",null,"L-3010107 Received October 25, 2013..  LC1369 removed from this ASR, paa, 11/4/13  Btl type is FUS, not GCC, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96762152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300147","Sample-Routine","Water","Groundwater","2013-05-07","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-393023119513701",null,"L-1300100 Received May 09, 2013..  S2437 split to 20131300206, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94424715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300060","Sample-Routine","Water","Groundwater","2013-06-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-360010088252901",null,"A-1780184 2 drops HCl in VOCs  H2S in sample  Actual sample collection time 0945 L-1780184 S2437 split to 20131780191, paa, 2/18/14  Samples were received chilled at the WHOI lab.","McNairy Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95010258","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305656","Sample-Routine","Water","Groundwater","2013-07-25","11:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364338119354602",null,"L-2110122 Received July 26, 2013..  NAWQA program code GWMSA added to ASR,paa,8/9/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95325321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300144","Sample-Routine","Water","Groundwater","2013-08-28","14:30:00","CDT",{"$nulls":4},76,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351111089512501",null,"A-2410228 2 drops HCl added to VOC  Actual radon collection time: 1631 CDT L-2410228 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96424621","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302858","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-290209096302701",null,"L-2420230 FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96369796","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300402","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-13","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-314204110224201",null,"L-2260076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96937465","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301688","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414233112174501",null,"L-2340074 X = Time on samples 1300, 1 GCV broken in cooler during shipping    Received August 21, 2013  Samples were received chilled at the WHOI lab.  X = Time on sample 1300",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible positive-pressure pump","NWIS-95682330","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300190","Sample-Routine","Water","Groundwater","2013-08-07","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363025082070401",null,"A-2250034 3 drops of HCL added to VOCs, H2S positive sniff test  Actual Radon time = 1311  H2S detected L-2250034 Received August 9, 2013  Samples were received chilled at the WHOI lab.  Updated date from 2013/08/06 per Kingsbury.  KB 3/7/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96472864","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300084","Sample-Routine","Water","Groundwater","2013-07-17","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311805085462401",null,"L-2000053 Received July 18, 2013..  S2437 split to 20132000301, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = You need station id on labels","Providence Sand","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96802205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400290","Sample-Routine","Water","Groundwater","2013-12-02","12:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365200119560001",null,"L-3380014 X=a PEST is a PEST, not a GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306287","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","PDT",{"$nulls":4},70,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380201",null,"L-2320034 One bottle has lid broken off, and all sample is missing  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96075341","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302045","Sample-Routine","Water","Surface Water","2013-07-23","09:10:00","EST",{"$nulls":14},"USGS-02350524",null,"L-2060191 Received July 24, 2013  Deleted LC 8252 per Rose.  KB 09/16/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107104896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300318","Sample-Routine","Water","Groundwater","2013-09-30","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-364912114041201",null,"L-2940041 Login delayed due to gov shutdown,ok log per Bexfield,paa,10/21/13    Received October 1,2013  File recvd late from TAL, paa  Login delayed due to gov shutdown, ok log per Bexfield, paa, 10/21/13    Received October 1, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96731658","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301282","Sample-Routine","Water","Groundwater","2013-09-18","11:00:00","CDT",{"$nulls":4},320,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305708087091201",null,"L-2620069 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96718991","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300051","Sample-Routine","Water","Groundwater","2013-07-09","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351253085105801",null,"A-1910015 Actual Sample Time 13:30 L-1910015 S2437 split to 20131910104, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94976882","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300065","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-325447080383601",null,"L-1970152 Received July 12, 2013..  S2437 split to 20131970170, paa, 3/13/14  Samples were received chilled at the WHOI lab.  Schedule 1792, not LC, paa",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94955288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305590","Sample-Routine","Water","Groundwater","2013-07-17","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-351556116404601",null,"L-1990171 S2437 split to 20131990210, paa, 3/14/14  1 bottle had no time, TAL  Only smpl identification on RADON is 0936, logged by paa from problem cooler, paa, 7/18/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95015806","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300734","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","CDT",{"$nulls":6},"Below land-surface datum",925,"feet",1025,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345021088572201",null,"L-2110047 Received July 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95377529","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-KY","USGS Kentucky Water Science Center","nwisky.01.01300436","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365200088210001",null,"L-2620048 X = FCC has no time, a PHARM is not a GCV    per Angie changed station ID and name  pwg  2013/09/26..  Sta ID changed to 365200088210001 per A. Crain, paa, 2/7/14  Samples were received chilled at the WHOI lab.  Updated SID from 365147088205702 and added station name per Crain.  KB 01/07/1",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96970314","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300477","Sample-Routine","Water","Groundwater","2013-09-11","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304921092402202",null,"L-2550097 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96471207","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301405","Sample-Routine","Water","Groundwater","2013-09-10","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",48,"feet",88,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-400026091242501",null,"L-2540101 ASRs recvd late & entered 1/21/14,paa  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96432919","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300956","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-24","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350012077131101",null,"L-2110205 Corrected ST to GWMSA, paa   Received July 27, 2013..  S2437 deleted from this ASR, invalid S2612 corrected to LC2612, paa, 8/9/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95362122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305613","Sample-Routine","Water","Groundwater","2013-07-25","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364312119592901",null,"L-2100107 S2437 & PEST split to separate ASR @1001, paa, 7/29/13    Received July 26, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95227896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305891","Sample-Routine","Water","Groundwater","2013-08-14","10:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372504",null,"L-2270210 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95531246","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300722","Sample-Routine","Water","Groundwater","2013-07-10","10:50:00","CDT",{"$nulls":6},"Below land-surface datum",1135,"feet",1185,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-331358088350001",null,"L-1920073 S2437 split to 20131920164, paa, 2/19/14  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95237088","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MT","USGS Montana Water Science Center","nwismt.01.01301628","Sample-Routine","Water","Surface Water","2013-08-28","10:40:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05014300",null,"L-2410104 Deleted 8252 per Rose.  KB 11/21/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107100098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306428","Sample-Routine","Water","Groundwater","2013-09-12","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363500120000001",null,"L-2590046 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098261","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305246","Sample-Routine","Water","Groundwater","2013-06-17","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-331211116185101",null,"L-1690111 X = btl type for Sch2437 is PEST, not GCV   Updated SID from 331200116180001 per Dugan.  KB 07/12/13  Sta id on btl 331200116180001 per WHOI, paa Samples were received chilled at the WHOI lab.  Updated SID from 331200116180001 per Dugan.  KB 07/12/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94758029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302483","Sample-Routine","Water","Groundwater","2013-06-26","15:15:00","MDT",{"$nulls":4},10,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-405159102444201",null,"L-1790275 S2437 split from 20131790260, paa, 2/18/14","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94803537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302861","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-291639097093901",null,"L-2400044 Received August 27, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300112","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352745084341201",null,"A-1970120 3 drops HCl in VOCs  Actual Sample Time = 13:08 L-1970120 X = Please do not use electrical tape on DOC sample    Received July 12, 2013  Updated SID from 352741084342001 and date from 20130712 per Kingsbury.  KB 3/7/14.. S2437 split to 20131970166, paa, 3/13/14  Samples were received chill",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96472245","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301866","Sample-Routine","Water","Groundwater","2013-08-12","18:00:00","EDT",{"$nulls":4},38,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-314858084194901",null,"A-2250046 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-95669666","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400293","Sample-Routine","Water","Groundwater","2013-12-04","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500120110001",null,"L-3400053 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776452","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300913","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","EDT",{"$nulls":4},164,"feet",null,200,"feet",220,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372454076512801",null,"L-2680168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96614817","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300248","Sample-Routine","Water","Groundwater","2013-07-24","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303001090274201",null,"L-2070070 Received July 25, 2013  Samples were received chilled at the WHOI lab.  X = Time sensitive time 1545",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95082821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301221","Sample-Routine","Water","Groundwater","2013-09-16","12:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345637076383501",null,"L-2630115 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96503293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300967","Sample-Routine","Water","Groundwater","2013-08-07","16:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343308077484501",null,"L-2240086 Received August 9, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95453906","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302936","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-11","10:30:00","CDT",{"$nulls":4},11,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-410959100582401",null,"L-1930218 S2437 split to 20131930249, paa, 2/20/14",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94915432","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300669","Sample-Routine","Water","Groundwater","2013-07-10","14:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-380027075410802",null,"L-1960087 Received July 12, 2013..  S2437 split to 20131960101, paa, 2/20/14  Even though samples lids were taped, some still leaked. JB 7/12/13 < 20cpm, TAL",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94893899","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302913","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-275725097562701",null,"L-2550106 ASRs recvd late & entered 1/21/14, paa  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96453689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305582","Sample-Routine","Water","Groundwater","2013-07-18","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363726119465201",null,"L-2030161 Received July 19, 2013..  S2437 split to 20132030169, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94984167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306275","Sample-Routine","Water","Groundwater","2013-08-21","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363337120070001",null,"L-2340269 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96158873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305545","Sample-Routine","Water","Groundwater","2013-07-09","10:10:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-381031121123901",null,"L-1930106 Received July 11, 2013..  S2437 split to 20131930243, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94888921","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400294","Sample-Routine","Water","Groundwater","2013-12-04","12:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365900120040001",null,"L-3400052 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776625","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300941","Sample-Routine","Water","Groundwater","2013-08-13","15:00:00","EDT",{"$nulls":6},"Below land-surface datum",52,"feet",67,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-394208082252201",null,"L-2270196 Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96559417","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305586","Sample-Routine","Water","Groundwater","2013-07-16","14:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363317119490401",null,"L-1990088 Btl type for S2437 is PEST not GVPEST, paa    Received July 17, 2013..  S2437 split to 20131990201, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985439","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301265","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-401002078254801",null,"L-2340287 GWMSA added, btl types corrected, paa, 8/22/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Other","NWIS-95667915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300839","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-371444080012701",null,"L-2400080 Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96295016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301261","Sample-Routine","Water","Groundwater","2013-09-24","15:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361252077074501",null,"L-2690102 4 bottles show sample date as 9/24/13. 9-23 will be used, per TestAm, paa..  ASR date corrected from 20130923 to 20130924 per Pointer, paa, 2/10/14  Samples were received chilled at the WHOI lab.  X= Date on sample 9/24/13..  ASR date corrected from 20130923 to 20130924 per Pointer, paa, 2",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96581152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306352","Sample-Routine","Water","Groundwater","2013-08-27","09:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364600119460001",null,"L-2410021 Received August 28,2013  2 of the bottles did not have station id #, date or time, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96374398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305210","Sample-Routine","Water","Groundwater","2013-06-12","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-341643116243101",null,"L-1640078 S2437 split to 20131640200, paa, 2/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94737449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300328","Sample-Routine","Water","Groundwater","2013-08-26","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-335825112435301",null,"L-2390103 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96280759","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300218","Sample-Routine","Water","Groundwater","2013-07-02","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332149113124601",null,"L-1860005 Received July 03, 2013..  S2437 split to 20131860104, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-94866036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","sample was dilutedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400021","Sample-Routine","Water","Groundwater","2013-10-29","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365649077233801",null,"L-3030199 Samples were received chilled at the WHOI lab..  WSC emailed for sample time, WHOI did not send btl label information, paa, 11/12/13..  time of 1200 added per Teunis, paa, 11/13/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96782434","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301262","Sample-Routine","Water","Groundwater","2013-09-25","10:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353749076333501",null,"L-2730030 Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96581607","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302676","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300413094402101",null,"L-2380135 Received August 23, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95676793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301264","Sample-Routine","Water","Groundwater","2013-09-26","10:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353605077483901",null,"L-2730034 Received September 27, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96582515","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306541","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-18","08:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-363700119550002",null,"L-2630170 Mising alk, WSC emailed, paa, 10/31/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96539013","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301267","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395625077585901",null,"L-2350258 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95668381","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400081","Sample-Routine","Water","Groundwater","2013-11-07","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-364151076571701",null,"L-3160061 Received November 08, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96838196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301390","Sample-Routine","Water","Groundwater","2013-09-17","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-433617092494301",null,"A-2610085 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6)- 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Exact time: 1315  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2610085 Samples were received chilled at the WH",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96492016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300611","Sample-Routine","Water","Groundwater","2013-09-26","10:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-434704096440701",null,"L-2950077 Logged from problem cooler per Joyce,delay due to gov shutdown,paa,10/22/13  Logged from problem cooler per Joyce, delay due to gov shutdown, paa, 10/22/13  Proposal added, paa  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96725909","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301268","Sample-Routine","Water","Groundwater","2013-09-24","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350420077084901",null,"L-2700188 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110392721","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306896","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-25","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351600116030002",null,"L-2700164 Received September 26, 2013   Updated SID from 351600116030001 per Vasquez.  KB 12/18/13  Samples were received chilled at the WHOI lab.   Updated SID from 351600116030001 per Vasquez.  KB 12/18/13  Updated SID from 351600116030001 per Vasquez.  KB 12/18/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-98339431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400024","Quality Control Sample-Field Replicate","Water","Groundwater","2013-10-30","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",264,"feet",420,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-370156077063801",null,"L-3040104 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96782906","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303430","Sample-Routine","Water","Groundwater","2013-08-12","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-431953088113701",null,"L-2250078 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113291811","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300819","Sample-Routine","Water","Groundwater","2013-08-28","13:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-391233075433102",null,"A-2410209 3 drops HCl in each VOC",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104235098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300121","Sample-Routine","Water","Groundwater","2013-07-30","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352554084193001",null,"A-2130055 4 drops of HCL added to VOCs  Actual Radon time = 1426 L-2130055 Received July 31, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95444799","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301483","Sample-Routine","Water","Groundwater","2013-09-30","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-445132093392101",null,"A-2940037 VOCs HAVE 5 DROPS HCL EACH VIAL (please lab filter schedule 2434)  GW-RADCHEM -- (6) - 1 LITER BOTLLES pres w/2mL NITRIC ACID <pH2  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-2940037 Login delayed due to gov shutdown, ok log per Terrio, paa, 10/21/13   Per btl labels, lab filter a",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96578141","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306272","Sample-Routine","Water","Groundwater","2013-08-22","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363900119500001",null,"L-2350235 X = Time on Sample 1030",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112097516","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301259","Sample-Routine","Water","Groundwater","2013-08-15","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-403325077242001",null,"L-2280187 GWMSA added to ASR, paa  Sta id on btl 403325077342001 per WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95517179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300716","Sample-Routine","Water","Groundwater","2013-07-29","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-381754075083601",null,"L-2120071 Received July 30, 2013",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95321354","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300670","Sample-Routine","Water","Groundwater","2013-07-11","10:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-381245075404001",null,"L-1970136 Received July 12, 2013..  S2437 split to 20131970167, paa, 3/13/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94894327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301300","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-404510077093801",null,"L-2400098 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96162973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300279","Sample-Routine","Water","Groundwater","2013-07-31","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334657113365501",null,"L-2130098 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95390601","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400078","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-06","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365147076343001",null,"L-3110102 STA ID changed per Alyssa M 11/26/13 GB  Samples were received chilled at the WHOI lab. STA ID changed per Alyssa M 11/26/13 GB",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96943034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301150","Sample-Routine","Water","Groundwater","2013-09-10","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342300077425401",null,"L-2550067 X = Date on bottles is 9-9-13  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96444391","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301340","Sample-Routine","Water","Groundwater","2013-09-11","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395804076084801",null,"L-2550048 ASRs recvd late & entered 1/21/14, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96431820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302648","Sample-Routine","Water","Groundwater","2013-09-17","10:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-414101094303802",null,"L-2610129 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96490010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300907","Sample-Routine","Water","Groundwater","2013-08-29","14:00:00","CDT",{"$nulls":6},"Below land-surface datum",1302,"feet",1368,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332056088420901",null,"L-2420353 Received August 30, 2013  Bottles are labeled 3/29/13 1400, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96362936","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303427","Sample-Routine","Water","Groundwater","2013-08-06","13:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-443810088311601",null,"L-2190092 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113291366","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301787","Sample-Routine","Water","Groundwater","2013-09-09","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385752112225301",null,"L-2530044 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96439288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301265","Sample-Routine","Water","Groundwater","2013-09-23","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351806077434501",null,"L-2700084 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110391352","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300317","Sample-Routine","Water","Groundwater","2013-09-23","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361023115114401",null,"L-2670013 ASR time 0900 (corrected from 9000), paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96731214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303371","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-440157089180501",null,"L-2060129 Received July 24, 2013..  PEST not recvd for this ASR, S2437 deleted, see 206-130 for pest, paa, 8/2/13  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113281717","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300821","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382843078363101",null,"L-2350198 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96294072","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300028","Sample-Routine","Water","Groundwater","2013-06-12","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302120087374201",null,"L-1650045 Received June 13, 2013..  S2437 split to 20131650195, paa, 2/14/14  Sample exceeds 72hrs per TAL, paa  Samples were received chilled at the WHOI lab.  X = Need to put label on outside of tube",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-94670165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300917","Sample-Routine","Water","Groundwater","2013-08-15","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345740089141601",null,"L-2310001 Received August 16, 2013  Updated UC from TN per Kingsbury.  KB 09/11/13  Updated UC from TN per Kingsbury.  KB 09/11/13  WHOI recvd smpl without ASR originally, ASR recvd 11/8, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96423304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300727","Sample-Routine","Water","Groundwater","2013-07-22","15:45:00","CDT",{"$nulls":6},"Below land-surface datum",545,"feet",625,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342111089124401",null,"L-2040214 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95312179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400461","Sample-Routine","Water","Groundwater","2013-12-11","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370100120060001",null,"L-3470072 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301153","Sample-Routine","Water","Groundwater","2013-09-11","15:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352200077230601",null,"L-2560051 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1315",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96445767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300141","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332833086203001",null,"L-2540048 X = Date on samples 9/7/2013   Updated SID from 332849086203501 per Gill.  KB 4/11/14  Sample date on bottle says 9/17/13, per TAL    ASRs recvd late & entered 1/21/14, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.    corrected station",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96927678","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300298","Sample-Routine","Water","Groundwater","2013-07-23","09:15:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-330420112034301",null,"L-2060173 Received July 24,2013..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  Samples were received chilled at the WHOI lab.  medium code corrected from WS to WG per Beisner, paa, 8/26/13  medium code corrected from WS to WG per Beisner, paa, 8/26/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95530139","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300866","Sample-Routine","Water","Groundwater","2013-09-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-370328080263101",null,"L-2600138 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96481995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300725","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-383756078455601",null,"L-2320018 Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95514802","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305671","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119385601",null,"L-2050179 Received July 23, 2013..  GWMSA added, WSC to verify, paa, 8/2/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab...  sta id changed to 85601 per Dugan, paa, 10/30/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95327078","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300397","Sample-Routine","Water","Groundwater","2013-07-17","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332916110510201",null,"L-1990162 Updated SID from 332927110511701 per Beisner.  KB 12/13/13..  S2437 split to 20131990209, paa, 3/14/14  Samples were received chilled at the WHOI lab.  Updated SID from 332927110511701 per Beisner.  KB 12/13/13  Updated SID from 332927110511701 per Beisner.  KB 12/13/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96936255","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300067","Sample-Routine","Water","Groundwater","2013-07-09","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-324829079533000",null,"L-1910021 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131910105, paa, 2/19/14  Corrected to schedule 1792, not lab code, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94956213","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400245","Sample-Routine","Water","Groundwater","2013-11-21","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365900120140001",null,"L-3290104 X=a PEST is a PEST, not a GCV     Received November 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-106775562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301174","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","CDT",{"$nulls":4},80,"feet",null,42,"feet",82,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375756088081201",null,"L-2380075 Received August 23, 2013  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95671290","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305662","Sample-Routine","Water","Groundwater","2013-07-24","10:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364259119385404",null,"L-2070171 GWMSA added to ASR, paa, 7/26/13   Received July 25, 2013  GWMSA added to ASR,paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95326202","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303379","Sample-Routine","Water","Groundwater","2013-07-31","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-450755088125301",null,"L-2130210 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113285154","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303375","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-451805088363101",null,"L-2110170 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283440","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300092","Sample-Routine","Water","Groundwater","2013-08-28","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315244085100401",null,"L-2410140 Updated SID from 315241085100501 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14","Tuscaloosa Group","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96811766","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300159","Sample-Routine","Water","Groundwater","2013-09-04","05:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324159087362001",null,"L-2480016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97173868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300275","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302832090064101",null,"L-2210134 WHOI ASR missing alkalinity, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95430725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302577","Sample-Routine","Water","Groundwater","2013-08-27","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-423846095141801",null,"L-2400168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96069579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301229","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354838076541201",null,"L-2630062 X = Time on samples 1000  Updated time from 100100 per Giorgino.  KB 8/5/15  Samples were received chilled at the WHOI lab.  X = Time on sample 1001",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96504205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300277","Sample-Routine","Water","Groundwater","2013-08-26","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-381704117031401",null,"L-2400093 Received August 27, 2013..  invalid med code GW corrected to WG, paa, 9/5/13  Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96427889","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300296","Sample-Routine","Water","Groundwater","2013-09-16","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-401115118301501",null,"L-2600153 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300242","Sample-Routine","Water","Groundwater","2013-07-09","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-334638112314501",null,"L-1910086 Updated SID from 334639112314801per Partin.  KB 08/07/13..  S2437 split to 20131910108, paa, 2/19/14  Samples were received chilled at the WHOI lab.  Updated SID from 334639112314801per Partin.  KB 08/07/13  Updated SID from 334639112314801per Partin.  KB 08/07/13  X = Time not on sample",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95232791","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300400","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322549111191601",null,"L-2110058 Received July 26, 2013..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  Samples were received chilled at the WHOI lab..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  medium code corrected from WS to WG per Beisner, paa, 8/26/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96936858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302225","Sample-Routine","Water","Groundwater","2013-09-16","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324816083290901",null,"L-2600158 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01300594","Sample-Routine","Water","Surface Water","2013-06-18","12:10:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-13210360",null,"L-1710091 ID user code per Romanok, paa, 6/20/13  Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107112487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301844","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313415084475201",null,"L-2270076 Received August 14, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95553116","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300790","Sample-Routine","Water","Groundwater","2013-08-20","09:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384630075524801",null,"A-2330078 1 drop HCl in VOC",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95663815","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300793","Sample-Routine","Water","Groundwater","2013-08-19","14:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383100076061103",null,"L-2320038 S1792 unclear, paa, ok'd to TALWA",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95664244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300733","Sample-Routine","Water","Groundwater","2013-07-25","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",597,"feet",637,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345002088374401",null,"L-2110051 Received July 26, 2013  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95376926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300217","Sample-Routine","Water","Groundwater","2013-06-26","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321846110592801",null,"L-1790022 Received June 27, 2013..  S2437 split to 20131790270, paa, 2/18/14  GWMSA added per NWQL ASRs, paa  GWMSA added, WSC to verify, paa, 7/3/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-94846967","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301213","Sample-Routine","Water","Groundwater","2013-08-28","11:00:00","CDT",{"$nulls":4},134,"feet",null,135,"feet",150,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-422448088041901",null,"L-2410083 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96272163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300100","Sample-Routine","Water","Groundwater","2013-07-09","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325627087043401",null,"L-1910053 X = Station ID not on btl's..  S2437 split to 20131910106, paa, 2/19/14  Samples were received chilled at the WHOI lab.  X = Station ID not on sample  Need label on outside of tube",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96813135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301067","Sample-Routine","Water","Groundwater","2013-08-28","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343400077292201",null,"L-2420329 Few samples had loose lids and leaked. COCs were not in plastic bag - soaked!, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96377142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302622","Sample-Routine","Water","Groundwater","2013-08-14","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-294040096542401",null,"L-2270120 Sta ID corrected from 542400 to 542401 per Ging,paa,9/10/13  Missing fields mandatory for WHOI,paa Samples were received chilled at the WHOI lab.  X = Only one FA bottle received  Sta ID corrected from 542400 to 542401 per Ging,paa,9/10/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95465651","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300127","Sample-Routine","Water","Groundwater","2013-07-23","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361610083581801",null,"A-2060161 3 drops of HCL added to VOCs  Actual Radon time = 12:52 L-2060161 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104108276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300421","Sample-Routine","Water","Groundwater","2013-08-05","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-331616111401101",null,"L-2180154 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-97270953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300202","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335128081250001",null,"L-2340223 Samples were received chilled at the WHOI lab.  Sch 1792 not LC1792, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95651065","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300991","Sample-Routine","Water","Groundwater","2013-09-04","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",53,"feet",63,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-432500082320001",null,"L-2480069 Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96408673","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300054","Sample-Routine","Water","Groundwater","2013-06-27","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351004088351501",null,"A-1820069 3 drops HCI in VOC's  Actual Radon time = 1015 L-1820069 Received Jun 28, 2013.. S2437 split to 20131820140, paa, 2/19/14  Updated SID from 351008088350601 per Kingsbury.  KB 3/7/14  Samples were received chilled at the WHOI lab..  Sta ID changed to 351004088351501 per Kingsbury,paa,3/13/1","Eutaw Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95010864","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400462","Sample-Routine","Water","Groundwater","2013-12-11","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700120090001",null,"L-3470073 Samples were received chilled at the WHOI lab..  sta id corrected from 9001 to 90001 per Dugan, paa, 2/10/14  Updated SID from 365700120090011 per Dugan.  KB 2/28/14  sta id corrected from 9001 to 90001 per Dugan, paa, 2/10/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777863","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300668","Sample-Routine","Water","Groundwater","2013-05-30","11:15:00","CDT",{"$nulls":6},"Below land-surface datum",139,"feet",161,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-313400091210001",null,"L-1510001 S2437 split to 20131510155, paa, 2/14/14  Btl type for S2255 is FUS, paa Samples were received chilled at the WHOI lab.  Sample is outside 72hrs per TAL, paa..  corrected LC1792 to Schedule 1792,paa,7/6/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94695044","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302679","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302207096050600",null,"L-2320028 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95678095","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300940","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",65,"feet",90,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-394257082362603",null,"L-2270194 Samples were received chilled at the WHOI lab..  smpl date changed from 20130812 to 20130813 per Runkle, WHOI notified, paa, 10/28/13","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96558923","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300311","Sample-Routine","Water","Groundwater","2013-08-20","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392212119223001",null,"L-2340238 Received August 21, 2013  Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Received August 21, 2013   Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Samples were received chilled at the WHOI lab.  Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Updated SID",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96574934","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300794","Sample-Routine","Water","Groundwater","2013-08-20","13:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-385023076013501",null,"A-2330080 3 drops HCl in VOC",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104234231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300164","Sample-Routine","Water","Groundwater","2013-08-12","15:00:00","CDT",{"$nulls":4},60,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350643089502001",null,"A-2320150 2 drops of HCl added to VOCs L-2320150 Recvd without ASR originally, paa    Recvd 8/14/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96462089","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302678","Sample-Routine","Water","Groundwater","2013-08-20","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302145095473901",null,"L-2340207 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95677660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300882","Sample-Routine","Water","Groundwater","2013-09-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-365525080564901",null,"L-2620055 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96550326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302209","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323255084141801",null,"L-2610071 X = A PHARM is not a GCV  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96700736","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306394","Sample-Routine","Water","Groundwater","2013-09-09","10:40:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364316119360102",null,"L-2540012 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96465878","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301267","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353257077285302",null,"L-2700186 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110392264","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300809","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384606075115801",null,"L-2400038 Received August 27, 2013",null,"Stable, normal stage","Routine sample",null,null,4044,"USGS parameter code 82398","Submersible jet pump",null,"Submersible positive-pressure pump","NWIS-96269660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300671","Sample-Routine","Water","Groundwater","2013-06-12","15:00:00","CDT",{"$nulls":6},"Below land-surface datum",650,"feet",700,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302825089042001",null,"L-1640162 Field alk added per Manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792, paa  S2437 split to 20131640201, paa, 2/14/14  verified PHARM not recvd for this ASR, LC9017 deleted, paa, 6/18/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94716983","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301788","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373900113130001",null,"L-2540111 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96439732","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305584","Sample-Routine","Water","Groundwater","2013-07-17","14:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363418119384201",null,"L-2000068 Received July 18, 2013..  S2437 split to 20132000303, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94986606","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301168","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","CDT",{"$nulls":4},60,"feet",null,55,"feet",65,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-391127088273501",null,"L-2330040 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95545955","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300670","Sample-Routine","Water","Groundwater","2013-06-12","10:00:00","CDT",{"$nulls":6},"Below land-surface datum",530,"feet",570,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310929088334101",null,"L-1650043 Received June 13, 2013    Lab codes not indicated as add or delete, LC's added, JNV  Field alk added per Manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792 per TALWA, time on btls is 10:00, paa    Updated time from 093500 per Manning.  KB 10/10/",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94716379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301227","Sample-Routine","Water","Groundwater","2013-09-18","09:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355220076371501",null,"L-2680110 X = Recvd without ASR logged in from problem cooler Sharon faxed 9/25/13, PG  ASR not recvd with smpls, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110390817","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400087","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-20","11:00:00","CST",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-443306094125501",null,"L-3250095 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96957832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301347","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-465926093354201",null,"A-2550072 VOCs HAVE   DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH2 LC1505 and LC2170 were shipped in a 2nd cooler  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1432  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-1",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96448332","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305587","Sample-Routine","Water","Groundwater","2013-07-16","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363316119473001",null,"L-1990090 Received July 17, 2013..  S2437 split to 20131990203, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300146","Sample-Routine","Water","Groundwater","2013-08-21","15:30:00","CDT",{"$nulls":4},71,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351448089421700",null,"A-2350039 2 drops HCl added to VOC L-2350039 Received August 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96425064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300146","Sample-Routine","Water","Groundwater","2013-05-06","10:45:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392937119452601",null,"L-1280031 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131280084, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94424307","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303643","Sample-Routine","Water","Groundwater","2013-08-28","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-445647091215301",null,"L-2420148 Samples were received chilled at the WHOI lab.  Some samples had leaked. COC and cooler wet per Test Am, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113297244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300102","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320431085315301",null,"L-2050150 X = Station id not on sample    Received July 23, 2013..  S2437 split to 20132050227, paa, 3/17/14   Updated SID from 320431085315401 per Gill.  KB 4/11/14  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/","Eutaw Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96813737","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300178","Sample-Routine","Water","Groundwater","2013-09-10","08:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351315089310501",null,"A-2540042 2 drops HCl added to VOCs L-2540042 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96461585","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300876","Sample-Routine","Water","Groundwater","2013-09-18","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380103076315901",null,"L-2620114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96502347","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300280","Sample-Routine","Water","Groundwater","2013-08-08","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",635,"feet",670,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-312144092401801",null,"L-2210320 Received August 09, 2013  WHOI ASR missing alkalinity, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95431180","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300743","Sample-Routine","Water","Groundwater","2013-07-23","16:15:00","CDT",{"$nulls":6},"Below land-surface datum",343,"feet",423,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341519088393901",null,"L-2060085 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95379978","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305610","Sample-Routine","Water","Groundwater","2013-07-16","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362921119335901",null,"L-1990089 Received July 17, 2013,  STA ID changed from 362621119335901 to 362921119335901 per Bennett GB..  S2437 split to 20131990202, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95074449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302479","Sample-Routine","Water","Groundwater","2013-06-24","14:20:00","MDT",{"$nulls":4},9.5,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-400237104500301",null,"L-1770009 LC not indicated as add or delete, LC added, JD..  S2437 split to 20131770130, paa, 2/18/14",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94804423","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302191","Sample-Routine","Water","Groundwater","2013-09-25","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312332084555101",null,"L-2690202 ASR missing mandatory alk, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96617648","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MT","USGS Montana Water Science Center","nwismt.01.01400725","Sample-Routine","Water","Groundwater","2014-04-30","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-470902113273501",null,"L-1210096 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97817497","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01402418","Sample-Routine","Water","Groundwater","2014-07-15","11:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343854106425601",null,"L-1970051 Samples were received chilled at the WHOI lab.  Sch 1792, not LC, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-98685606","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400284","Sample-Routine","Water","Surface Water","2014-04-15","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214655255",null,"A-1070012 10 min time offset",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97702315","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400378","Sample-Routine","Water","Surface Water","2014-04-16","10:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0208524090",null,"A-1070135 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97747492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401154","Sample-Routine","Water","Surface Water","2014-06-11","13:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02095181",null,"L-1690057 Received June17, 2014",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98459973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401199","Sample-Routine","Water","Surface Water","2014-06-11","16:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0212430653",null,"L-1690092 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98477301","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01402087","Sample-Routine","Water","Groundwater","2014-05-14","12:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320642106440401",null,"L-1360089 Received May 15, 2014  Radon completely unlabeled, only sample recvd with this ASR, WSC notified, paa, 5/16/14    Received May 15, 2014  Samples leaked a little, per TAL  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98372907","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01400471","Sample-Routine","Water","Surface Water","2014-06-11","10:20:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02165200",null,"L-1690120 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98442001","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400735","Sample-Routine","Water","Surface Water","2014-05-13","10:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02085500",null,"L-1360081 Received May 15, 2014..  ASR date changed from 20140512 to 20140513 per Cassy P,paa,6/6/14",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97955558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400798","Sample-Routine","Water","Groundwater","2014-01-13","15:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380302121203201",null,"L-0150012 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-112099668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-01-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404355","Sample-Routine","Water","Groundwater","2014-08-18","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361207121075501",null,"L-2330026 Received August 20, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-105560148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01400898","Sample-Routine","Water","Groundwater","2014-07-31","13:00:00","EST",{"$nulls":6},"Below land-surface datum",null,null,170,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382556078565401",null,"L-2130077 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98823072","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-06","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01401162","Quality Control Sample-Field Replicate","Water","Groundwater","2014-08-07","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-364917078275401",null,"L-2310074 recvd warm 8/11, ok to login per Moberg recvd 8/18, PG Chilled containers received warm at 9.1   Degrees C  Recvd warm 8/11   Ok to login per Moberg recvd 8/18, PG Chilled containers received warm at 9.1   Degrees C  X=added date & time per Erik S.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99150235","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-20","sample was warm when receivedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404280","Sample-Routine","Water","Groundwater","2014-08-11","13:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-353800120380001",null,"L-2250106 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106884975","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401189","Sample-Routine","Water","Surface Water","2014-06-10","14:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214265808",null,"L-1690115 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98465895","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01403520","Sample-Routine","Water","Groundwater","2014-08-20","10:00:00","MDT",{"$nulls":13},"USGS - Colorado Water Science Center","USGS-365802105313101",null,"L-2340267 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-104282190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402295","Sample-Routine","Water","Groundwater","2014-07-15","11:00:00","CST",{"$nulls":4},230,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-441948088094901",null,"L-1970139 S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab.  X=no date on sample","Ordovician-Cambrian Systems","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-113366845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01402046","Sample-Routine","Water","Surface Water","2014-06-11","09:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02207435",null,"A-1680209 4 Drops HCl",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98396156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402801","Sample-Routine","Water","Groundwater","2014-05-02","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-323925117044001",null,"L-1250099 X=per Sue D. ok to log in warm cooler 8.4c, PG, 5/5/14 Chilled containers received warm at 8.4   Degrees C  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-112105973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-08","sample was warm when receivedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01402554","Sample-Routine","Water","Groundwater","2014-07-17","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-293116098334101",null,"L-1990028 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-98712576","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01400502","Sample-Routine","Water","Groundwater","2014-08-18","09:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Michigan Water Science Center","USGS-461500085550001",null,"L-2320070 Received August 19, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Other","NWIS-98954097","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01401127","Sample-Routine","Water","Groundwater","2014-08-26","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392929077530202",null,"L-2400141 Received August 27,2014  Received August 27, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-99284451","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01401662","Sample-Routine","Water","Groundwater","2014-09-03","14:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-384902090451201",null,"A-2470115 Pest Sample  Environmental Sample: VOCs have 3 drops HCl in each vial  GW Radchem - (6) 1L bottles, preserved with 2mL NA  Radon sample collected @ 1505  University of Miami Tritium Laboratory  1 LITER BOTTLE FOR TRITIUM ANALYSIS",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-99209953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-06","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402327","Sample-Routine","Water","Groundwater","2014-07-10","09:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-443921089152001",null,"L-1950012 Received July 11, 2014",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113370647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01400540","Sample-Routine","Water","Groundwater","2014-08-11","10:00:00","CDT","2014-08-11","10:01:59","CDT",{"$nulls":8},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-442209100225001",null,"L-2240087 Modified inorg ASR to log organic smpls per Tyler, paa, 8/12/14  S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.  X=need to put sample information on outside of tube.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Grab sample","NWIS-99167722","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-ME","USGS Maine Water Science Center","nwisma.01.01401150","Sample-Routine","Water","Groundwater","2014-08-20","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",35,"feet",45,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-453849067521001",null,"L-2340172 Added USEPA agency code, GB12/19/14   Received August 21, 2014  Added USEPA agency code, GB12/19/14  Added USEPA agency code, GB12/19/14  Samples were received chilled at the WHOI lab.  X=date on sample 8/20/14   Added USEPA agency code, GB12/19/14   Date missing in mandatory field Time =(","Stratified Deposits, Undifferentiated","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-99123417","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404630","Sample-Routine","Water","Groundwater","2014-09-15","11:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-383916122473501",null,"L-2610121 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106888016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01403521","Sample-Routine","Water","Groundwater","2014-08-27","11:00:00","MDT",{"$nulls":13},"USGS - Colorado Water Science Center","USGS-360027106063401",null,"L-2410097 Samples were received chilled at the WHOI lab.","Santa Fe Group","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-99201965","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01400646","Sample-Routine","Water","Groundwater","2014-09-09","10:00:00","EST",{"$nulls":4},200,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-341249081320100",null,"L-2530014 proj acct chg per F.Falls, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-99256420","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401474","Sample-Routine","Water","Groundwater","2014-08-26","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362336079270001",null,"L-2460143 Received August 29, 2014  Proposal corrected, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99190780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-05","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402569","Sample-Routine","Water","Groundwater","2014-04-22","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-331710116415401",null,"L-1190090 Received April 26, 2014 Chilled containers received warm at 7.6   Degrees C..  recvd warm 3/26, ok log per Dugan, PG  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-112105051","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-01","sample was warm when receivedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404830","Sample-Routine","Water","Groundwater","2014-09-24","10:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420003",null,"L-2680032 S2755 added per Mathany,S1306 deleted and S4443 added per Justin K,paa,9/25/14..  S4443 deleted per Mathany/Rose, paa, 9/30/14  Samples were received chilled at the WHOI lab.  X=improper sample container - sample sent in 40mL btl..  proposal corrected to CL14NAWCA per Mathany, paa, 12/8/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99371220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402565","Sample-Routine","Water","Groundwater","2014-04-25","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-325122116562101",null,"L-1180173 RECEIVED APRIL 25, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112104378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01400468","Sample-Routine","Water","Groundwater","2014-07-21","12:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-321245091495501",null,"L-2030134 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-98765004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404086","Sample-Routine","Water","Groundwater","2014-08-06","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700121580001",null,"A-2200034 DROPS OF VOC ACID= 3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106883755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401183","Sample-Routine","Water","Surface Water","2014-06-11","08:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02146470",null,"L-1690040 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98464836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401171","Sample-Routine","Water","Surface Water","2014-06-09","10:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02097280",null,"A-1630207 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98462713","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01400163","Sample-Routine","Water","Groundwater","2014-08-12","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351113089513401",null,"A-2260153 WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-2260153 X=time on sample 1400..  pesticide left as is per NAWQA,paa,8/15/14  Updated time from 100000 per Kingsbury.  KB 9/2/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-99072399","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01503555","Sample-Routine","Water","Groundwater","2015-07-16","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314348094421401",null,"L-1980183 Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-101354024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-07-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01501719","Quality Control Sample-Field Replicate","Water","Groundwater","2015-01-13","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361700119340001",null,"L-0140025 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112108390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-01-23","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01501441","Quality Control Sample-Field Replicate","Water","Groundwater","2015-05-14","11:05:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-382915100544201",null,"L-1350149 X=no station id on PHARM or PEST",null,"Stable, normal stage","Routine sample",null,null,8040,"USGS parameter code 82398","Spigot",null,"Jet pump","NWIS-100825791","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-21","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500742","Sample-Routine","Water","Groundwater","2015-04-16","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-292420081084001",null,"L-1100037 Received April 17, 2015  H2S - Yes Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-109648933","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-26","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01503101","Sample-Routine","Water","Groundwater","2015-09-02","16:10:00","PDT",{"$nulls":4},70.5,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-462824119140801",null,"L-2530076 FED EX LATE DELIVERY",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101838290","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-16","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01500200","Sample-Routine","Water","Groundwater","2015-03-23","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392900115560001",null,"L-0830027 invalid S2170 corrected to S2710 per btls, NAWQA notified, paa, 3/24/15",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible positive-pressure pump","NWIS-100330615","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-03-28","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600557","Quality Control Sample-Field Replicate","Water","Groundwater","2015-12-09","13:20:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390300121030001",null,"A-3450174 DROPS OF VOC ACID=5",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112116069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503724","Quality Control Sample-Field Replicate","Water","Groundwater","2015-04-27","12:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-355447119250001",null,"A-1190049 DROPS OF VOC ACID = 3",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-104668921","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-02","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600018","Sample-Routine","Water","Groundwater","2015-10-07","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-410800122180001",null,"L-2860037 Received October 09, 2015  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106933995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-10-17","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01505145","Sample-Routine","Water","Groundwater","2015-08-12","14:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-341100118092001",null,"L-2260040 Changed account number to GP15ZG00FC1G500 per G. Bennett, ACW, 8/18/15  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106925646","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-21","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01502492","Sample-Routine","Water","Groundwater","2015-03-03","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-360900119170001",null,"L-0630091 Samples were received chilled at the WHOI lab.  per ALS, time on btl 1330, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-104664235","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-03-05","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01500325","Sample-Routine","Water","Groundwater","2015-04-21","09:35:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-433322112564301",null,"L-1130152 S1380 deleted and S4436 added per Maimer,D. Rose verified,paa,4/27/15",null,"Not determined","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-100499982","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-29","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503041","Sample-Routine","Water","Groundwater","2015-04-01","10:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361400119460001",null,"L-0920079 ASR missing WSC contact, paa  Samples were received chilled at the WHOI lab.  Smdugan added, S1792 changed to S1979 by ALS, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104666390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600595","Sample-Routine","Water","Groundwater","2015-12-17","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392400120570001",null,"A-3520032 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112117167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-28","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500783","Sample-Routine","Water","Groundwater","2015-08-11","16:00:00","CDT",{"$nulls":4},11.5,"feet",null,14.5,"feet",19.5,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-384646090375501",null,"A-2240121 Alternate contact-Kelly Warner(klwarner)/217-328-09727   drops HCL for VOC  Alternate contact - Kelly Warner, klwarner@usgs.gov 217-328-9725. Acidified with HNO3. Acidified with HNO3. RADCHEM - acidified HNO3","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101521623","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-15","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01504670","Sample-Routine","Water","Groundwater","2015-08-04","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322137095243601",null,"L-2180112 X=ok to log in warm samples per Patty Ging. Chilled containers received warm at 8.1   Degrees C  Samples were received chilled at the WHOI lab.  X=ok to login warm samples per Patty Ging Chilled containers received warm at 8.1   Degrees C",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-101802945","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-11","sample was warm when receivedsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600372","Sample-Routine","Water","Groundwater","2015-11-16","09:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391400121080001",null,"L-3220048 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112115511","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-11-20","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01501213","Sample-Routine","Water","Groundwater","2015-08-20","09:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384428075355701",null,"L-2330155 Samples were received chilled at the WHOI lab.  Updated SID from 384637075153201 per Cruz.  KB 10/23/15",null,"Not applicable","Not applicable",null,null,8030,"USGS parameter code 82398","Grab sample at water-supply tap",null,"Submersible positive-pressure pump","NWIS-101635450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01505446","Sample-Routine","Water","Groundwater","2015-09-14","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373600121170001",null,"L-2600060 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106932931","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-24","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500975","Sample-Routine","Water","Surface Water","2015-08-26","13:00:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05543500",{"$nulls":3},"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-101745018","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500413","Sample-Routine","Water","Surface Water","2015-05-07","10:30:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05541510",null,"L-1320087 X=no btl types on GCC, GCV, OXW, PEST, PHARM and TOC, no schedule or lab codes on btls   Received May 09, 2015..  Emailed WSC contact, missing proposal # for LC 9030,3406,9031,4440, & 8099, ACW, 5/13/15 Added proposal # CL15023, ACW, 5/19/15",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-100743136","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-14","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01502491","Sample-Routine","Water","Groundwater","2015-03-04","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-360000119270001",null,"L-0690046 X=ok to log  per Hansen, KS, 3/10/15   received warm 3/9 Chilled containers received warm at 7.8   Degrees C  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-104664056","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-03-14","sample was warm when receivedsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01504666","Sample-Routine","Water","Groundwater","2015-07-28","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-285513099492801",null,"L-2100076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-101803591","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-01","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600448","Sample-Routine","Water","Groundwater","2015-12-03","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-351300119150001",null,"A-3380067 DROPS OF VOC ACID=3",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106938874","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-08","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01500329","Sample-Routine","Water","Groundwater","2015-04-21","11:21:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-433401112551001",null,"L-1130148 S1380 deleted and S4436 added per Maimer,D. Rose verified,paa,4/27/15",null,"Not determined","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-100500192","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-29","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601397","Sample-Routine","Water","Groundwater","2016-07-20","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-471928118412501",null,"L-2030129 X=no time on DOC & GCVs  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105284288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01603038","Sample-Routine","Water","Groundwater","2016-08-03","12:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431037090043401",null,"L-2439605 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-113537035","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01600135","Sample-Routine","Water","Groundwater","2016-08-17","10:00:00","EST",{"$nulls":4},10.6,"feet",null,11,"feet",16,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-340158080574601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105540115","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01605758","Sample-Routine","Water","Groundwater","2016-08-10","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385455120481601",null,"L-2250084 No tape on cap, cap loose - No leak or loss of sample Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112126612","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01606331","Quality Control Sample-Field Replicate","Water","Groundwater","2016-09-14","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382931120350401",null,"L-2590034 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112129403","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01603920","Quality Control Sample-Field Replicate","Water","Groundwater","2016-05-18","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-354300118330001",null,"L-1410034 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-108899351","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01602333","Sample-Routine","Water","Groundwater","2016-03-15","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392800121150001",null,"L-0770037 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112122338","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01603730","Sample-Routine","Water","Groundwater","2016-06-16","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","TX001-352134101324007",null,"L-1690154 Changed Station ID to current per P. Ging. JPC 8/29/16  Samples were received chilled at the WHOI lab. Changed Station ID to current per P. Ging. JPC 8/29/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105054980","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01602031","Sample-Routine","Water","Groundwater","2016-01-25","13:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-283512099350301",null,"L-0260020 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103564259","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-01-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01604344","Sample-Routine","Water","Groundwater","2016-07-13","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362021102045401",null,"L-1960214 One bottle for LC 1364 was empty upon receipt At ALS. Lid had broken  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105237336","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601853","Sample-Routine","Water","Groundwater","2016-03-03","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373500120510001",null,"L-0700018 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-106944141","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-18","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01604120","Sample-Routine","Water","Groundwater","2016-05-23","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-393300120490001",null,"L-1470016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-112125681","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01604709","Sample-Routine","Water","Groundwater","2016-08-01","12:30:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351347106370301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105514161","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01601401","Sample-Routine","Water","Groundwater","2016-01-14","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-281546099234601",null,"L-0150099 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103269301","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-01-20","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-OR","USGS Oregon Water Science Center","nwisor.01.01600406","Sample-Routine","Water","Groundwater","2016-08-01","08:00:00","PDT",{"$nulls":4},275,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-455351119205601",null,"L-2150218 Corrected UC from OK to OR per ASR.  KB 2/2/17",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Other","NWIS-110443298","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01601452","Sample-Routine","Water","Groundwater","2016-07-13","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Missouri Water Science Center","USGS-373936094105601",null,"L-1960266 X=time on btls is 1030. Changed Time from 1200 to 1030 per J. Wilson. JPC 9/7/16  Samples were received chilled at the WHOI lab.  Sch 1792 changed to 1979 due to high solids  X=time on container is 1030. Changed Time from 1200 to 1030 per J. Wilson. JPC 9/7/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105134868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01601040","Quality Control Sample-Field Replicate","Water","Groundwater","2016-04-28","10:00:00","CDT",{"$nulls":13},"USGS-District Water-Quality Lab, Little Rock, Arkansas","USGS-371412090575601",null,"L-1200065 Changed proposal number from CL16NAW16 to CL16NAWMO. 5/2/2016 MEC  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-103785915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-06","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701143","Sample-Routine","Water","Groundwater","2016-12-15","10:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333855096542701",null,"L-3510056 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106525957","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01605762","Quality Control Sample-Field Replicate","Water","Groundwater","2016-08-08","09:50:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391523120422401",null,"L-2240035 FED EX LATE DELIVERY  No tape, cap loose - no leak or loss of smaple Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-112127357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01601538","Sample-Routine","Water","Groundwater","2016-08-30","09:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-261537080141601",null,"L-2440030 Samples were received chilled at the WHOI lab. Result 77035, rejected on 12/21/21, because a national-scale QC evaluation for groundwater indicated that contamination bias likely resulted in relatively common detections taht do not represent environmental conditions.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109261196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701147","Sample-Routine","Water","Groundwater","2016-12-12","12:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333826097213601",null,"L-3480090 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106528456","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701151","Sample-Routine","Water","Groundwater","2016-12-05","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323011096543001",null,"L-3410097 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106529713","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01600885","Sample-Routine","Water","Groundwater","2016-08-01","11:00:00","EDT",{"$nulls":4},18,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-423004083463000",null,"L-2150092 SCH1792 changed to 1979 due to high solids  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4047,"USGS parameter code 82398","Submersible gear pump",null,"Submersible gear pump","NWIS-105441875","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01602055","Sample-Routine","Water","Groundwater","2016-03-08","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-291744097303800",null,"L-0700007 Changed Station ID to current per P. Ging. JPC 3/28/16  Samples were received chilled at the WHOI lab.. Changed Station ID to current per P. Ging. JPC 3/28/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103563337","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01700212","Sample-Routine","Water","Groundwater","2016-11-16","12:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-485930122431001",null,"L-3230003 X=received #1 of 4437 vials broken.  Added Schedules 4436 and 4437 per Huffman. 11/21/2016 mec  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-106271902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-11-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601613","Sample-Routine","Water","Groundwater","2016-02-02","09:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390500121000001",null,"L-0340045 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112120118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01600971","Quality Control Sample-Field Replicate","Water","Groundwater","2016-08-10","10:00:00","EST",{"$nulls":4},18,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384637075153201",null,"L-2240168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-105482064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01602331","Sample-Routine","Water","Groundwater","2016-03-17","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391400120420001",null,"L-0780045 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112121967","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-OR","USGS Oregon Water Science Center","nwisor.01.01600412","Sample-Routine","Water","Groundwater","2016-08-11","08:00:00","PDT",{"$nulls":4},0,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-451754120142101",null,"L-2250195 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Other","NWIS-110446096","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01706101","Sample-Routine","Water","Groundwater","2017-06-27","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-342100119180001",null,"L-1810226 Please do not put tape on GCC cap  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115684005","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800068","Sample-Routine","Water","Groundwater","2017-10-19","09:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382600121305501",null,"L-2930055 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110972986","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800679","Sample-Routine","Water","Groundwater","2017-12-20","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424025076321001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-109376846","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-12-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01701467","Sample-Routine","Water","Groundwater","2017-09-26","10:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-403107109323501",null,"L-2700080 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Grab sample","NWIS-108870300","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800396","Sample-Routine","Water","Groundwater","2017-11-20","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-422937076531401",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-109213260","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-12-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01706425","Sample-Routine","Water","Groundwater","2017-07-12","12:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341400118550001",null,"L-1950088 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115684264","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01700703","Sample-Routine","Water","Groundwater","2017-06-12","13:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-413708076131901",null,"L-1640176 X=time on bottles is 1300",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107854272","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707839","Quality Control Sample-Field Replicate","Water","Groundwater","2017-09-20","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385200120000001",null,"L-2650153 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115691020","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800222","Sample-Routine","Water","Groundwater","2017-11-01","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425854075285701",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-109113327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-11-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01702189","Sample-Routine","Water","Groundwater","2017-02-02","09:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340033117204001",null,"L-0340023 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109468228","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-02-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700477","Sample-Routine","Water","Groundwater","2017-06-26","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394233075045402",null,"L-1790057 X=GCV not labeled 1 2 or 3  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107953031","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01700667","Sample-Routine","Water","Groundwater","2017-06-22","09:30:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-424129114230201",null,"L-1740012 Use ball point not felt tip. See X=for details. X=station id, date & time smeared on second RU, second FA & first 4436 GCV. Cannot read.",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-107974893","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707110","Sample-Routine","Water","Groundwater","2017-08-10","12:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382650121101501",null,"L-2230115 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-110966473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703756","Sample-Routine","Water","Groundwater","2017-06-07","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302646099481501",null,"L-1590298 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108587112","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01702006","Sample-Routine","Water","Groundwater","2017-01-24","13:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340700117240001",null,"L-0270006 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109466780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-02-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01701208","Sample-Routine","Water","Groundwater","2017-07-11","10:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381943110401701",null,"L-1930097 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-108427218","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MA","USGS Massachusetts Water Science Center","nwisma.01.01701126","Sample-Routine","Water","Groundwater","2017-08-08","13:00:00","EDT",{"$nulls":4},10,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420322072391801",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-108465888","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703752","Sample-Routine","Water","Groundwater","2017-06-14","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305714103114001",null,"L-1660025 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108593470","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01703943","Sample-Routine","Water","Groundwater","2017-09-08","12:00:00","MDT",{"$nulls":13},"USGS - Colorado Water Science Center","USGS-395458108325002",{"$nulls":3},"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Submersible positive-pressure pump","NWIS-108724377","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01700138","Sample-Routine","Water","Groundwater","2017-08-16","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351113089513401",null,"L-2300038 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-108568946","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800042","Sample-Routine","Water","Groundwater","2017-10-11","13:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-333130114394001",null,"L-2860115 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-125522990","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-19",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800006","Sample-Routine","Water","Groundwater","2017-10-04","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384140121375001",null,"L-2790064 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110971967","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701737","Sample-Routine","Water","Groundwater","2017-03-09","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-291839099382801",null,"L-0690081 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-107060405","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-03-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01701196","Sample-Routine","Water","Groundwater","2017-09-18","15:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-430549092272301",null,"L-2620301 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108853903","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01800225","Sample-Routine","Water","Groundwater","2017-10-31","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-293405098394201",null,"L-3050118 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-109121064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700462","Sample-Routine","Water","Groundwater","2017-06-21","09:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394321075015701",null,"L-2059602 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107897803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01706100","Sample-Routine","Water","Groundwater","2017-06-27","13:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341700119090001",null,"L-1810227 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115683743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802283","Sample-Routine","Water","Groundwater","2018-03-21","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-343038117341701",null,"L-0820079 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-115700251","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01804603","Sample-Routine","Water","Groundwater","2018-06-26","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345200120290001",null,"L-1780140 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115958138","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01805849","Sample-Routine","Water","Groundwater","2018-09-11","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-372700118440001",null,"L-2570170 Add District Contact RHKENT to ASR.  KMS, 9/17/18  Sample arrived with some exterior fracturing, but according to WHO1 staff, there appears to be no effect on sample. (no leaking) Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-118316488","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01900340","Sample-Routine","Water","Groundwater","2018-10-22","09:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-352350117451601",null,"L-2990162 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118325129","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800928","Sample-Routine","Water","Groundwater","2018-07-30","12:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-465113099552701",null,"L-2180004 Received August 4,2018  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111575986","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01801656","Sample-Routine","Water","Groundwater","2018-03-13","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-293745098162001",null,"L-0730036 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110505318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01900115","Sample-Routine","Water","Groundwater","2018-11-07","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-432349075565301",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-112232282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01800895","Sample-Routine","Water","Groundwater","2018-09-04","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393807075030401",null,"L-2480071 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible centrifugal pump","NWIS-111694969","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01804966","Sample-Routine","Water","Groundwater","2018-07-25","13:50:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370700121370001",null,"L-2080180 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-118318042","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802948","Sample-Routine","Water","Groundwater","2018-04-02","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361123121040801",null,"L-1638702 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115703726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-04-27","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01804258","Sample-Routine","Water","Groundwater","2018-05-22","15:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-343004117380801",null,"L-1430051 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116130960","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01900339","Sample-Routine","Water","Groundwater","2018-10-22","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-351125116374901",null,"L-2990165 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-118324869","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01801827","Quality Control Sample-Field Replicate","Water","Groundwater","2018-02-12","09:50:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345418117100901",null,"L-0470022 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116127002","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-02-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800936","Sample-Routine","Water","Groundwater","2018-08-14","10:50:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-474007102272501",null,"L-2280014 X=added user code from shipping state label  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111577084","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01804970","Sample-Routine","Water","Groundwater","2018-07-23","15:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374000121520001",null,"L-2080183 Added TMATHANY to ASR as District Contact based on another ASR received in the same cooler.  KMS, 7/30/18  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-118322780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01800429","Sample-Routine","Water","Groundwater","2018-07-26","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-443042092570401",null,"L-2080211 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111361649","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802218","Sample-Routine","Water","Groundwater","2018-03-07","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-344434117200401",null,"L-0680135 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-115698307","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800727","Sample-Routine","Water","Groundwater","2018-07-19","10:30:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-475802103381501",null,"L-2198704 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111319733","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-07-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01801156","Sample-Routine","Water","Groundwater","2018-08-06","15:10:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-485608122320501",null,"L-2299610 NWQL IT work for CSR 13769.  The ASRNO was written by the contract lab incorrectly on this ASR. It should have been 20182198507.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-111979244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01804326","Sample-Routine","Water","Groundwater","2018-05-30","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-344303117242001",null,"L-1520093 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124193814","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000384","Sample-Routine","Water","Groundwater","2019-10-30","17:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-263000081430001",null,"L-3040028 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118426758","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906033","Sample-Routine","Water","Groundwater","2019-07-11","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380526121150201",null,"L-1970128 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118744475","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02000586","Sample-Routine","Water","Groundwater","2019-11-25","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-420925075534001",null,"L-3310069 RECEIVED NOV 27 2019.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-118203162","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-12-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02000270","Sample-Routine","Water","Groundwater","2019-10-29","08:45:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424702075253201",null,"L-3030163 X = ASR's were sent in wrong cooler.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-118068446","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000468","Sample-Routine","Water","Groundwater","2019-11-19","09:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-283700080500001",null,"L-3240067 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118450151","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01901655","Sample-Routine","Water","Groundwater","2019-02-12","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-400027122081601",null,"L-0460060 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118296821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-02-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01905688","Sample-Routine","Water","Groundwater","2019-06-26","11:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394855123144801",null,"L-1790053 GCV bottles changed to improper preservation, JR.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118761379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-06","improper preservationsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902074","Quality Control Sample-Field Replicate","Water","Groundwater","2019-06-18","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420910070530901",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116942222","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-06-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01902269","Sample-Routine","Water","Groundwater","2019-07-23","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USEPA-390502081475404",null,"L-2050176 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-117665226","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000408","Sample-Routine","Water","Groundwater","2019-11-13","14:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-262649080053901",null,"L-3180073 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118431787","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02000054","Sample-Routine","Water","Groundwater","2019-10-07","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-420540076030701",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117928393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902328","Sample-Routine","Water","Groundwater","2019-07-31","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-415820071082401",null,"L-2140312 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117364242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000372","Sample-Routine","Water","Groundwater","2019-10-30","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-264500081260000",null,"L-3040029 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118424240","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01902600","Sample-Routine","Water","Groundwater","2019-09-16","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-442859073250301",null,"L-2600181 X= FU and FCC labels were switched in the field.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117779060","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ME","USGS Maine Water Science Center","nwisma.01.01903043","Sample-Routine","Water","Groundwater","2019-09-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-450232069525101",null,"L-2690202 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117855566","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01903025","Sample-Routine","Water","Groundwater","2019-03-20","12:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-362658119192801",null,"L-1008707 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118031072","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-04-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01900724","Sample-Routine","Water","Groundwater","2019-08-05","15:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-371052089052501",null,"L-2180145 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Other","NWIS-117569458","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-10",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01900104","Sample-Routine","Water","Groundwater","2019-09-18","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323408080411009",null,"L-2620209 Samples were received chilled at the WHOI lab. L-2620209 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117780943","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902836","Sample-Routine","Water","Groundwater","2019-09-12","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420434071225001",null,"L-2600207 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117739588","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-KY","USGS Kentucky Water Science Center","nwisky.01.01900227","Sample-Routine","Water","Groundwater","2019-08-22","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375454086454401",null,"L-2350081 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Other","NWIS-117806454","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IN","USGS Indiana Water Science Center","nwisin.01.01901085","Sample-Routine","Water","Groundwater","2019-06-12","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380751085543601",null,"MM-57071A",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Mulitple samplers used","NWIS-117734755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-06-19",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02001727","Sample-Routine","Water","Groundwater","2020-06-30","16:30:00","EDT",{"$nulls":6},"Below land-surface datum",195,"feet",305,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332141081591901",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-119309695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001963","Sample-Routine","Water","Groundwater","2020-09-17","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-444721074453501",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119714854","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02004079","Sample-Routine","Water","Groundwater","2020-09-02","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340900117550001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-120699022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100728","Sample-Routine","Water","Groundwater","2020-12-01","12:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-372617120530201",null,"L-3390100 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122457028","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-12-12",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02002101","Sample-Routine","Water","Groundwater","2020-09-14","07:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-422752078064801",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119826131","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02001703","Sample-Routine","Water","Groundwater","2020-06-29","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",110,"feet",120,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332221081584602",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-119296315","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02004363","Sample-Routine","Water","Groundwater","2020-09-21","09:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373755120501501",null,"L-2690100 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122449141","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100512","Sample-Routine","Water","Groundwater","2020-11-18","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-405200122150001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122573811","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-11-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001964","Sample-Routine","Water","Groundwater","2020-02-10","09:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-334510116173601",null,"L-0440008 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-120715748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-02-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003097","Sample-Routine","Water","Groundwater","2020-06-23","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384224121261401",{"$nulls":3},"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-120691574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02002105","Sample-Routine","Water","Groundwater","2020-09-08","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-443329075412101",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119827271","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02002104","Sample-Routine","Water","Groundwater","2020-09-23","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-441256074190401",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119826983","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003088","Sample-Routine","Water","Groundwater","2020-06-17","08:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-333519116135401",null,"L-1750171 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-120709536","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02000382","Sample-Routine","Water","Groundwater","2020-08-04","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",145,"feet",140,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302109092523101",null,"L-2180146 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-119411689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001518","Sample-Routine","Water","Groundwater","2020-01-13","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-335344116272501",null,"L-0150086 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120717840","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-01-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100489","Sample-Routine","Water","Groundwater","2020-11-02","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373519121020901",null,"L-3110016 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122453560","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-11-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02200154","Sample-Routine","Water","Groundwater","2021-10-26","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385306120592301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124684464","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-10-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102890","Sample-Routine","Water","Groundwater","2021-04-12","13:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373828120444001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-123268668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-04-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02102007","Sample-Routine","Water","Groundwater","2021-09-22","08:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-423324074061601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-122414599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102889","Sample-Routine","Water","Groundwater","2021-04-12","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374526120475501",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-123268355","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-04-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02103813","Sample-Routine","Water","Groundwater","2021-05-24","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-350600118270002",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-123275465","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02103815","Sample-Routine","Water","Groundwater","2021-05-25","15:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-353500118280001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-123275955","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02103045","Sample-Routine","Water","Groundwater","2021-04-27","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371722120192401",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-123271171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-05-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.02100228","Sample-Routine","Water","Groundwater","2021-05-18","09:00:00","CST",{"$nulls":4},20,"feet",null,22,"feet",27,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-430728088132801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122907324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-05-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02104681","Sample-Routine","Water","Groundwater","2021-07-20","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371000121460001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124427044","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101865","Sample-Routine","Water","Groundwater","2021-07-28","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-422126079024801",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-121686574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-08-04","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02200443","Sample-Routine","Water","Groundwater","2021-11-17","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382137120403401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124682450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-11-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02200015","Sample-Routine","Water","Groundwater","2021-10-06","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394258121515301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124411392","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-10-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02102122","Quality Control Sample-Field Replicate","Water","Groundwater","2021-09-01","12:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-332215081575201",null,null,"Midville Aquifer System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122375293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101904","Sample-Routine","Water","Groundwater","2021-07-28","07:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431553077564301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-121770056","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-08-04","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.02100224","Sample-Routine","Water","Groundwater","2021-05-26","08:30:00","CST",{"$nulls":4},18,"feet",null,21.1,"feet",26.1,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-421633088125801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122405515","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02104434","Sample-Routine","Water","Groundwater","2021-06-28","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390058121260001",{"$nulls":3},"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-125824495","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02300268","Sample-Routine","Water","Groundwater","2022-11-15","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382444121123301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125799868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-11-22","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203488","Sample-Routine","Water","Groundwater","2022-03-31","12:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-352206119121201",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-125840121","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-04-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.02200512","Sample-Routine","Water","Groundwater","2022-04-05","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375541076514301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-123457522","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-04-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.02200059","Sample-Routine","Water","Groundwater","2022-06-29","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332833086203001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-123848561","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203913","Sample-Routine","Water","Groundwater","2022-05-24","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382410122311501",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125237682","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-05-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02201626","Quality Control Sample-Field Replicate","Water","Groundwater","2022-06-29","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",202,"feet",283,"feet",null,null,"U.S. Geological Survey-Water Resources Discipline","USGS-332146081590601",null,null,"Midville Aquifer System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124095421","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02300374","Quality Control Sample-Field Replicate","Water","Groundwater","2022-11-30","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384024121281301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125797071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-12-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02204138","Sample-Routine","Water","Groundwater","2022-05-24","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340747117170501",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-123749686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.02200632","Sample-Routine","Water","Groundwater","2022-06-28","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-400350074451001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124002899","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02300174","Sample-Routine","Water","Groundwater","2022-10-20","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364824121302301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125797778","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-10-29","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203908","Sample-Routine","Water","Groundwater","2022-05-18","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382306122480601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125236788","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-05-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.02200838","Sample-Routine","Water","Groundwater","2022-06-16","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380022079025601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124017236","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02202680","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-14","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341300119040001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-125238787","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-03-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.02300039","Sample-Routine","Water","Groundwater","2022-11-02","14:00:00","MST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-435557116411701",{"$nulls":3},"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124666948","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-11-08","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02204670","Sample-Routine","Water","Groundwater","2022-07-14","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385500120000001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-125707197","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-07-23","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201691","Quality Control Sample-Field Replicate","Water","Groundwater","2022-08-15","10:01:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431023075311201",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124822893","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-19","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02201625","Sample-Routine","Water","Groundwater","2022-02-01","12:00:00","PST",{"$nulls":13},"USGS - California Water Science Center","USGS-351913118463701",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125819763","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-02-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02305203","Sample-Routine","Water","Groundwater","2023-07-20","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-363928119401701",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125944496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-07-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02305200","Sample-Routine","Water","Groundwater","2023-07-19","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-363418119384201",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125943880","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-07-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW02-VP-D002-052004-0","Sample","Air","Ambient Air","2004-05-20","17:30:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW02",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047850053.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-05-25",{"$nulls":3},4.2,"ppb",null,null,"STORET"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW04-VP-D003-052004-0","Sample","Air","Ambient Air","2004-05-23","08:14:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW04",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047851442.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-05-27",{"$nulls":3},7,"ppb",null,null,"STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-95153R-gwdb","Sample-Routine","Water","Groundwater","2011-10-07","11:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-77503","CLEAN HARBORS AZ CH-4",{"$nulls":4},33.4421758,-112.0904453,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-492546135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2011-10-13",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-95153R-gwdb/results/492546135/resdetectqntlmts","Method Detection Level",2,"ug/L",null,"2015-12-04T11:54:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120342.CHEM","Sample-Routine","Other",null,"2013-12-16","08:40:00","EST",{"$nulls":4},85,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-53577",64409,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5248041,-112.0816008,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725055126","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120342.CHEM/results/725055126/resdetectqntlmts","Laboratory Reporting Level",0.02,"mg/L",null,"2018-05-10T17:39:51","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122647-gwdb","Sample-Routine","Water","Groundwater","2013-12-16","12:40:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79223","ADEQ MW-103",{"$nulls":4},32.2459961,-109.8361039,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882425","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122647-gwdb/results/490882425/resdetectqntlmts","Lower Reporting Limit",0.05,"mg/L",null,"2015-11-30T18:12:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122642-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","08:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490809263","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122642-gwdb/results/490809263/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:19:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122645-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","07:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79232","ADEQ MW-112",{"$nulls":4},32.2458997,-109.8357839,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490775166","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122645-gwdb/results/490775166/resdetectqntlmts","Lower Reporting Limit",0.04,"mg/L",null,"2015-11-30T16:50:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120314.CHEM","Sample-Routine","Other",null,"2013-08-01","02:05:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-52553",62913,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.52445,-112.0817647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725053568","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120314.CHEM/results/725053568/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2018-05-10T17:39:27","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120521R-gwdb","Sample-Other","Water","Groundwater","2013-10-30","11:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490866254",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-11-03",{"$nulls":6},"2015-11-30T17:58:12","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120441R-gwdb","Sample-Other","Water","Groundwater","2013-08-01","14:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802929",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-04",{"$nulls":6},"2015-11-30T17:15:38","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120493R-gwdb","Sample-Other","Water","Groundwater","2013-10-30","09:35:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490803032",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-11-03",{"$nulls":6},"2015-11-30T17:15:41","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122569-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","15:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79262","ADEQ MW-102",{"$nulls":4},32.26686,-109.8468753,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490884469","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122569-gwdb/results/490884469/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:13:57","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122142-gwdb","Sample-Routine","Water","Groundwater","2014-03-10","09:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-59281","WCP-71M",{"$nulls":4},33.4976731,-112.1465367,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490871589",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-14",{"$nulls":6},"2015-11-30T18:02:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120500R-gwdb","Sample-Other","Water","Groundwater","2014-03-20","08:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490803281","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120500R-gwdb/results/490803281/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122442-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","08:52:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79222","ADEQ MW-102",{"$nulls":4},32.2461081,-109.8364322,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491018211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-26",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122442-gwdb/results/491018211/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:49","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122114-gwdb","Sample-Routine","Water","Groundwater","2014-03-05","10:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57166","F&B MW-3(259)",{"$nulls":4},33.4982861,-112.1430889,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490806213",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-12",{"$nulls":6},"2015-11-30T17:17:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120476.CHEM","Sample-Routine","Other",null,"2014-03-18","03:32:00","EST",{"$nulls":4},105,"ft",{"$nulls":5},9517,"2014-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-58794",79327,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5245131,-112.0836091,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725058131","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120476.CHEM/results/725058131/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2018-05-10T17:40:55","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121777-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","11:46:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491008192","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121777-gwdb/results/491008192/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:12:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122417-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","15:54:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491019357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122417-gwdb/results/491019357/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:18:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121778-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","08:56:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490869848","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121778-gwdb/results/490869848/resdetectqntlmts","Lower Reporting Limit",0.02,"mg/L",null,"2015-11-30T18:00:15","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132466-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","13:58:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79224","ADEQ MW-104",{"$nulls":4},32.2460894,-109.8361219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490811282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-18",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132466-gwdb/results/490811282/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:52","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122457-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","09:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79223","ADEQ MW-103",{"$nulls":4},32.2459961,-109.8361039,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490808395","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122457-gwdb/results/490808395/resdetectqntlmts","Lower Reporting Limit",0.02,"mg/L",null,"2015-11-30T17:19:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120262.CHEM","Sample-Routine","Other",null,"2014-01-27","12:45:00","EST",{"$nulls":4},85,"ft",{"$nulls":5},9517,"2014-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-52553",62913,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.52445,-112.0817647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725050760","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120262.CHEM/results/725050760/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2018-05-10T17:38:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120299.CHEM","Sample-Routine","Other",null,"2014-03-19","11:20:00","EST",{"$nulls":4},120,"ft",{"$nulls":5},9517,"2014-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-56984",72801,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5246358,-112.0828885,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725052829","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120299.CHEM/results/725052829/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2018-05-10T17:39:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147021-gwdb","Sample-Routine","Water","Groundwater","2015-06-26","07:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552101810","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-07-10",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147021-gwdb/results/552101810/resdetectqntlmts","Lower Reporting Limit",0.02,"mg/L",null,"2016-05-12T02:44:42","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147531-gwdb","Sample-Routine","Water","Groundwater","2015-03-19","11:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-80307","PETREE-S - MW-201",{"$nulls":4},33.4993778,-112.0740361,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552086892","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Xenco Laboratories","2015-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147531-gwdb/results/552086892/resdetectqntlmts","Lower Reporting Limit",5,"ug/L",null,"2016-05-12T02:38:53","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147107-gwdb","Sample-Routine","Water","Groundwater","2015-01-05","19:15:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80121","ADEQ MW-1R",{"$nulls":4},33.4316522,-112.0748403,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552082684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-01-10",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147107-gwdb/results/552082684/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:37:47","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146998-gwdb","Sample-Routine","Water","Groundwater","2015-05-28","12:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79869","ADEQ MW-9",{"$nulls":4},33.9350128,-114.0081956,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552158519","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146998-gwdb/results/552158519/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:11:13","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148340-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","13:35:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551977568","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148340-gwdb/results/551977568/resdetectqntlmts","Lower Reporting Limit",0.01,"mg/L",null,"2016-05-12T01:32:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148817-gwdb","Sample-Routine","Water","Groundwater","2015-09-22","14:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-80427","LDS CHURCH WELL",{"$nulls":4},34.1545439,-109.9757011,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552061747","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-09-30",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148817-gwdb/results/552061747/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",null,"2016-05-12T02:27:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150563-gwdb","Sample-Routine","Water","Groundwater","2015-09-24","12:50:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80590","MW-1",{"$nulls":4},33.4929136,-113.1616156,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552116037","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150563-gwdb/results/552116037/resdetectqntlmts","Lower Reporting Limit",0.01,"mg/L",null,"2016-05-12T02:51:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146145-gwdb","Sample-Routine","Water","Groundwater","2015-03-05","12:18:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-61601","IRA-24",{"$nulls":4},32.2873592,-111.0120722,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552100852","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-13",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146145-gwdb/results/552100852/resdetectqntlmts","Method Detection Level",2,"ug/L",null,"2016-05-12T02:44:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148333-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","10:33:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552135737","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148333-gwdb/results/552135737/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:58:30","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148949-gwdb","Sample-Other","Water","Groundwater","2015-10-22","15:28:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-67698","WOC-207S",{"$nulls":4},33.4774144,-112.1471392,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552171557","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148949-gwdb/results/552171557/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:14:39","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146147-gwdb","Sample-Routine","Water","Groundwater","2015-03-17","12:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-67120","SJ-MW-2",{"$nulls":4},32.2739831,-111.003225,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551973150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-21",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146147-gwdb/results/551973150/resdetectqntlmts","Method Detection Level",2,"ug/L",null,"2016-05-12T01:29:47","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147254-gwdb","Sample-Other","Water","Groundwater","2015-03-20","13:13:00","MST",{"$nulls":11},"MISC","MISC",null,"21ARIZ_WQX-59290","SOUTHERN & MILL MW-4L",{"$nulls":4},33.3948558,-111.9383539,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552052013","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Xenco Laboratories","2015-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147254-gwdb/results/552052013/resdetectqntlmts","Lower Reporting Limit",5,"ug/L",null,"2016-05-12T02:22:59","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148977-gwdb","Sample-Routine","Water","Groundwater","2015-11-19","13:08:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552140120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148977-gwdb/results/552140120/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:01:09","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148932-gwdb","Sample-Other","Water","Groundwater","2015-10-23","13:13:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65184","WOC-202S",{"$nulls":4},33.4840147,-112.1323092,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552171638","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148932-gwdb/results/552171638/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:14:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155734.CHEM","Sample-Routine","Other",null,"2016-08-22","12:03:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59278",81145,{"$nulls":4},34.5618417,-112.4861667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676215438","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-08-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155734.CHEM/results/676215438/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2017-11-03T10:14:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156444.CHEM","Sample-Routine","Other",null,"2016-10-26","05:11:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58746",79221,{"$nulls":4},32.2460864,-109.8363083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676176066","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156444.CHEM/results/676176066/resdetectqntlmts","Laboratory Reporting Level",0.004,"mg/L",null,"2017-11-03T10:08:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-150953.CHEM","Sample-Routine","Other",null,"2016-03-02","02:18:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59189",80593,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4927864,-113.1616206,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707988885","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-03-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-150953.CHEM/results/707988885/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-03-13T10:39:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155740.CHEM","Sample-Routine","Other",null,"2016-05-02","04:05:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59308",81171,{"$nulls":4},34.5618889,-112.4869556,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676261047","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-05-09",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155740.CHEM/results/676261047/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2017-11-03T10:24:29","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-151679-gwdb","Sample-Other","Water","Groundwater","2016-03-16","09:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-70421","ADEQ MW-209S",{"$nulls":4},33.4653172,-112.1377258,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552079203","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-151679-gwdb/results/552079203/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:36:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155757.CHEM","Sample-Routine","Other",null,"2016-09-07","10:04:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59197",80601,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4929,-113.162135,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707990174","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-09-11",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155757.CHEM/results/707990174/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-03-13T10:40:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156920.CHEM","Sample-Routine","Other",null,"2016-12-06","09:39:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59199",80603,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4930581,-113.1623814,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993810","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156920.CHEM/results/707993810/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-03-13T10:41:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156880.CHEM","Sample-Routine","Other",null,"2016-11-21","11:32:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59320",81183,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},34.5619778,-112.4865694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707992063","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156880.CHEM/results/707992063/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",null,"2018-03-13T10:40:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-154958.CHEM","Sample-Routine","Other",null,"2016-05-25","04:10:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59010",79950,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},34.90249,-110.1636969,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707989112","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-154958.CHEM/results/707989112/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2018-03-13T10:40:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156919.CHEM","Sample-Routine","Other",null,"2016-12-05","11:29:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59195",80599,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4931642,-113.1622069,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993733","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156919.CHEM/results/707993733/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-03-13T10:41:15","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150943-gwdb","Sample-Routine","Water","Groundwater","2016-03-01","10:50:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80494","CCM_MW-4",{"$nulls":4},35.1906006,-109.4332819,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552095149","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-06",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150943-gwdb/results/552095149/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",null,"2016-05-12T02:40:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156874.CHEM","Sample-Routine","Other",null,"2016-11-22","10:16:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59312",81175,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},34.5621472,-112.4865639,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707991613","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156874.CHEM/results/707991613/resdetectqntlmts","Laboratory Reporting Level",200,"ug/L",null,"2018-03-13T10:40:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB10552.CHEM","Sample-Routine","Other",null,"2017-09-11","11:40:00","EST",{"$nulls":11},9750,"2018 NPL","AMEC","AZDEQ_WPD-54647",62289,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4427639,-112.0774722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-718067412","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB10552.CHEM/results/718067412/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-04-24T09:59:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB10553.CHEM","Sample-Routine","Other",null,"2017-09-11","02:15:00","EST",{"$nulls":11},9750,"2018 NPL","AMEC","AZDEQ_WPD-54644",62286,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4431667,-112.07725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-718067503","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB10553.CHEM/results/718067503/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-04-24T09:59:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB03830.CHEM","Sample-Routine","Other",null,"2017-08-16","12:57:00","EST",{"$nulls":4},224.6,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES",null,"AZDEQ_WPD-48036",57704,{"$nulls":4},34.2285256,-111.3335314,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676134468","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"J",null,224.6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB03830.CHEM/results/676134468/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2017-11-03T09:09:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-157539.CHEM","Sample-Routine","Other",null,"2017-02-22","12:45:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","URS CONSULTANTS","AZDEQ_WPD-53577",64409,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5248041,-112.0816008,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725064693","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX","2017-02-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-157539.CHEM/results/725064693/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-05-10T17:42:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB10597.CHEM","Sample-Routine","Other",null,"2017-09-21","10:15:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","HGC","AZDEQ_WPD-61741",81447,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.5559542,-112.4720974,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-719003928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"XENCO LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB10597.CHEM/results/719003928/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",null,"2018-04-25T10:23:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB08129.CHEM","Sample-Routine","Other",null,"2017-09-15","08:00:00","EST",{"$nulls":11},9749,"2018-WQARF Samples",null,"AZDEQ_WPD-55792",69219,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.303385,-111.0357892,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-703248013","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB08129.CHEM/results/703248013/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-02-21T11:01:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB16630.CHEM","Sample-Routine","Other",null,"2018-11-13","08:51:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52798",63336,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2018136,-110.9687664,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-776068861","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB16630.CHEM/results/776068861/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2019-02-13T18:29:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB16623.CHEM","Sample-Routine","Other",null,"2018-11-13","03:11:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-61958",81627,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2021361,-110.969325,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-776069134","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB16623.CHEM/results/776069134/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2019-02-13T18:29:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB09658.CHEM","Sample-Routine","Other",null,"2018-02-15","01:01:00","EST",{"$nulls":11},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-58425",78221,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4330189,-112.0983989,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725089621","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB09658.CHEM/results/725089621/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-05-11T10:33:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18600.CHEM","Sample-Routine","Water","Groundwater","2018-06-25","03:55:00","EST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58634",78974,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.5163472,-112.0651667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789230550","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18600.CHEM/results/789230550/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-13T09:47:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB15163.CHEM","Sample-Routine","Other",null,"2018-11-15","11:35:00","EST",{"$nulls":4},105,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-762126828","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB15163.CHEM/results/762126828/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-12-17T17:33:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB16856.CHEM","Sample-Routine","Other",null,"2018-08-30","10:06:00","EST",{"$nulls":4},113,"ft",{"$nulls":5},9750,"2018 NPL","JACOBS ENGINEERING","AZDEQ_WPD-61647",81390,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.939051,-110.302279,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-776946954","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"L",null,113,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"XENCO LABORATORIES - TEMPE",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB16856.CHEM/results/776946954/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",null,"2019-02-26T09:35:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB16842.CHEM","Sample-Routine","Other",null,"2018-08-30","01:33:00","EST",{"$nulls":4},115,"ft",{"$nulls":5},9750,"2018 NPL","JACOBS ENGINEERING","AZDEQ_WPD-61786",81482,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.9395694,-110.3068917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-776945890","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"L",null,115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"XENCO LABORATORIES - TEMPE",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB16842.CHEM/results/776945890/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",null,"2019-02-26T09:34:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB15167.CHEM","Sample-Routine","Other",null,"2018-11-15","12:35:00","EST",{"$nulls":4},145,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-762127148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,145,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB15167.CHEM/results/762127148/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-12-17T17:33:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB09657.CHEM","Sample-Routine","Other",null,"2018-02-14","01:36:00","EST",{"$nulls":4},145,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725089541","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,145,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB09657.CHEM/results/725089541/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-05-11T10:33:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25021.CHEM","Sample-Routine","Water","Groundwater","2019-11-19","11:21:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52694",63124,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2023014,-110.9699608,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-827752636","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25021.CHEM/results/827752636/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-03-13T11:23:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28853.CHEM","Sample-Routine","Other","Groundwater","2019-10-02","01:45:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856014611","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28853.CHEM/results/856014611/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2020-09-10T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26148.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","02:00:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62400",81882,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4270989,-112.0871484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832562029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26148.CHEM/results/832562029/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-07T11:05:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25014.CHEM","Sample-Routine","Water","Groundwater","2019-11-20","11:06:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52698",63128,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016983,-110.9688897,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-827753289","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25014.CHEM/results/827753289/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-03-13T11:23:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28863.CHEM","Sample-Routine","Other","Groundwater","2019-10-03","10:21:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856015291","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28863.CHEM/results/856015291/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2020-09-10T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29984.CHEM","Sample-Routine","Water","Groundwater","2019-04-11","10:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62356",81852,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7372168,-112.0058959,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872413256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29984.CHEM/results/872413256/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2021-01-19T10:34:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29078.CHEM","Sample-Routine","Other","Groundwater","2019-12-11","11:08:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859910056","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29078.CHEM/results/859910056/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",null,"2020-10-14T17:37:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29070.CHEM","Sample-Routine","Other","Groundwater","2019-12-11","11:53:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909536","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29070.CHEM/results/859909536/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",null,"2020-10-14T17:37:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26152.CHEM","Sample-Routine","Water","Groundwater","2019-12-30","10:10:00","MST",{"$nulls":4},160,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62401",81883,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4289567,-112.0911729,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832562819","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},160,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26152.CHEM/results/832562819/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-07T11:05:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26150.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","01:10:00","MST",{"$nulls":4},99,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62400",81882,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4270989,-112.0871484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832561950","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},99,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26150.CHEM/results/832561950/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-07T11:05:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28864.CHEM","Sample-Routine","Other","Groundwater","2019-10-02","12:16:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856015359","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28864.CHEM/results/856015359/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2020-09-10T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29975.CHEM","Sample-Routine","Water","Groundwater","2019-01-30","12:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62352",81848,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7362426,-112.0103577,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872412590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29975.CHEM/results/872412590/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2021-01-19T10:33:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29974.CHEM","Sample-Routine","Water","Groundwater","2019-01-30","01:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62354",81850,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7359976,-112.0104707,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872412516","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29974.CHEM/results/872412516/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2021-01-19T10:33:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18593.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","08:10:00","EST",{"$nulls":4},396,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50531",60646,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2178769,-110.8320742,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-788806821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,396,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18593.CHEM/results/788806821/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2019-06-07T09:23:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB24942.CHEM","Sample-Routine","Water","Groundwater","2019-09-18","02:11:00","MST",{"$nulls":4},215,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-51313",61442,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4276056,-112.088,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-824334282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},215,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB24942.CHEM/results/824334282/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-02-25T09:36:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29086.CHEM","Sample-Routine","Other","Groundwater","2019-12-12","11:13:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859910574","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29086.CHEM/results/859910574/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",null,"2020-10-14T17:37:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29257.CHEM","Sample-Routine","Water","Groundwater","2020-08-27","10:20:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52690",63120,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016586,-110.9696389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860053622","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29257.CHEM/results/860053622/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2020-10-22T13:18:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28324.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","03:50:00","MST",{"$nulls":4},84,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58629",78969,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5111917,-112.0715472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},84,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28324.CHEM/results/850123022/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29269.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","10:27:00","MST",{"$nulls":4},42,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50199",62104,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4877681,-111.9961122,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860613171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,42,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29269.CHEM/results/860613171/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29281.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","08:22:00","MST",{"$nulls":4},90.7,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56542",71385,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900806,-111.9946153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860614424","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: H1.",null,90.7,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29281.CHEM/results/860614424/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28313.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","11:35:00","MST",{"$nulls":4},292,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49516",59448,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089208,-112.0741147,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122208","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},292,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28313.CHEM/results/850122208/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32894.CHEM","Sample-Routine","Water","Groundwater","2020-10-15","06:28:00","MST",{"$nulls":4},142,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58622",78962,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3597333,-111.8042472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905983878","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,142,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32894.CHEM/results/905983878/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-08-03T09:45:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26370.CHEM","Sample-Routine","Water","Groundwater","2020-03-13","11:00:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62400",81882,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4270989,-112.0871484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839247400","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26370.CHEM/results/839247400/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-22T09:30:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29336.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","01:41:00","MST",{"$nulls":4},265,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62052",81663,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4730179,-112.0239066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860619087","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,265,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29336.CHEM/results/860619087/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29300.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","01:02:00","MST",{"$nulls":4},205,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62247",81750,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4750136,-112.0119411,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616201","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,205,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29300.CHEM/results/860616201/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29779.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","01:05:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29779.CHEM/results/871506896/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29325.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","06:59:00","MST",{"$nulls":4},210,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62478",81925,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4863199,-112.0079,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860618125","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,210,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29325.CHEM/results/860618125/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28106.CHEM","Sample-Routine","Water","Groundwater","2020-04-01","11:40:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-39780",46086,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0762236,-114.5983106,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849876081","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28106.CHEM/results/849876081/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-24T11:03:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29337.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","08:25:00","MST",{"$nulls":4},96.8,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56542",71385,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900806,-111.9946153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860619230","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,96.8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29337.CHEM/results/860619230/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30006.CHEM","Sample-Routine","Water","Groundwater","2020-12-08","11:25:00","MST",{"$nulls":11},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52798",63336,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018136,-110.9687664,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-873226183","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30006.CHEM/results/873226183/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2021-01-26T09:19:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26357.CHEM","Sample-Routine","Water","Groundwater","2020-03-09","12:30:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-51313",61442,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4276056,-112.088,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839244743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26357.CHEM/results/839244743/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-22T09:29:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32860.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","08:16:00","MST",{"$nulls":4},170,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-46649",46639,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3781028,-111.8241681,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905981761","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,170,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32860.CHEM/results/905981761/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-08-03T09:45:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30005.CHEM","Sample-Routine","Water","Groundwater","2020-12-08","03:15:00","MST",{"$nulls":11},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52862",63334,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2014664,-110.9687608,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-873226092","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30005.CHEM/results/873226092/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2021-01-26T09:19:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29692.CHEM","Sample-Routine","Water","Groundwater","2020-09-22","01:38:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-54780",66601,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495395,-111.9792992,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871301074","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29692.CHEM/results/871301074/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-12-22T12:17:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29711.CHEM","Sample-Routine","Water","Groundwater","2020-09-23","08:01:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-40430",46748,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4945336,-111.9822153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871302523","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29711.CHEM/results/871302523/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-12-22T12:17:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28105.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","01:10:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59152",80430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1514111,-109.9719722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805918","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28105.CHEM/results/849805918/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28320.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","11:50:00","MST",{"$nulls":4},81,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55118",67537,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5117814,-112.0741767,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},81,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28320.CHEM/results/850122726/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28670.CHEM","Sample-Routine","Water","Groundwater","2020-07-21","09:57:00","MST",{"$nulls":4},330,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62099",81698,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3595803,-110.8348695,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-853891398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,330,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28670.CHEM/results/853891398/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2020-08-10T10:43:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30166.CHEM","Sample-Routine","Water","Groundwater","2020-10-30","04:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61656",81398,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.150759,-109.9739609,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30166.CHEM/results/874608431/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28319.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","12:25:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55124",67543,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5090942,-112.0743069,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122652","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28319.CHEM/results/850122652/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33056.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","08:57:00","MST",{"$nulls":4},52,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56549",71392,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4950161,-111.9809294,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916454814","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,52,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33056.CHEM/results/916454814/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35346.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-22","12:00:00","MST",{"$nulls":4},101,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63023",82387,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.879323,-111.7356152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994634738","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,V1.",null,101,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35346.CHEM/results/994634738/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2023-12-04T10:15:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33338.CHEM","Sample-Routine","Water","Groundwater","2021-08-31","08:04:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-57683",75250,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2551146,-114.1457726,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916468941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5,V1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33338.CHEM/results/916468941/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:15:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36492.CHEM","Sample-Routine","Water","Groundwater","2021-08-24","09:23:00","MST",{"$nulls":4},219.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62910",82280,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387596,-112.1868051,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937425425","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},219.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36492.CHEM/results/937425425/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:37:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36429.CHEM","Sample-Routine","Water","Groundwater","2021-12-17","10:15:00","MST",{"$nulls":4},77,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937421851","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},77,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36429.CHEM/results/937421851/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2022-05-03T12:36:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35315.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","03:55:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62982",82348,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356701,-110.9417204,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994633276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35315.CHEM/results/994633276/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2023-12-04T10:15:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35732.CHEM","Sample-Routine","Water","Groundwater","2021-12-01","02:59:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47014",56626,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048912,-112.1498029,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994415718","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35732.CHEM/results/994415718/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-01T09:39:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33058.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","09:57:00","MST",{"$nulls":4},55,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62543",81978,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934,-111.9863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916454962","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,55,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33058.CHEM/results/916454962/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33337.CHEM","Sample-Routine","Water","Groundwater","2021-08-31","10:15:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62877",82248,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2554558,-114.1465214,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916468849","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5,V1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33337.CHEM/results/916468849/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:15:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35435.CHEM","Sample-Routine","Water","Groundwater","2021-10-19","12:46:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62996",82362,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3668245,-110.9403282,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-932823218","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35435.CHEM/results/932823218/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2022-03-18T10:56:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43754.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","05:10:00","MST",{"$nulls":4},120,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63285",82603,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934158,-112.0072961,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992951810","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},120,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43754.CHEM/results/992951810/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33082.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","08:04:00","MST",{"$nulls":4},175,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50235",60338,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3779486,-111.8246017,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916457477","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,175,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33082.CHEM/results/916457477/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35327.CHEM","Sample-Routine","Water","Groundwater","2021-12-07","08:48:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62978",82344,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358918,-110.9416598,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994634118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35327.CHEM/results/994634118/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:15:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35730.CHEM","Sample-Routine","Water","Groundwater","2021-12-01","08:13:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63058",82392,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482178,-112.1488252,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994415643","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35730.CHEM/results/994415643/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-01T09:39:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34153.CHEM","Sample-Routine","Water","Groundwater","2021-11-29","10:45:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62669",82074,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.255782,-114.146513,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994133200","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8,N1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34153.CHEM/results/994133200/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-29T09:06:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33226.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","08:11:00","MST",{"$nulls":4},220,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916457847","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,V1,L5.",null,220,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33226.CHEM/results/916457847/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47796.CHEM","Sample-Routine","Water","Groundwater","2021-10-20","03:25:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63156",82475,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5275306,-112.0805145,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-979419185","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47796.CHEM/results/979419185/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-06-26T10:50:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34168.CHEM","Sample-Routine","Water","Groundwater","2021-11-29","11:45:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62671",82076,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.256313,-114.14668,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994134310","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8,D1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34168.CHEM/results/994134310/resdetectqntlmts","Laboratory Reporting Level",8,"ug/L",null,"2023-11-29T09:06:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33150.CHEM","Sample-Routine","Water","Groundwater","2021-09-09","04:09:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62861",82232,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2561218,-110.0236611,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916462483","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33150.CHEM/results/916462483/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2021-10-19T11:13:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34769.CHEM","Sample-Routine","Water","Groundwater","2021-12-06","03:01:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62871",82242,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2533371,-110.0342156,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626897","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34769.CHEM/results/994626897/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:14:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33228.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","08:16:00","MST",{"$nulls":4},260,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916458064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: P,  | QA FLAGS: E8,D1,V1,L5.",null,260,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33228.CHEM/results/916458064/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2021-10-19T11:12:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33318.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","05:31:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62639",82046,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0188168,-110.6841705,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916500638","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33318.CHEM/results/916500638/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2021-10-21T10:57:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43502.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","08:10:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63284",82602,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4929743,-112.0074929,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-966047417","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43502.CHEM/results/966047417/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-01-30T10:12:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40316.CHEM","Sample-Routine","Water","Groundwater","2021-01-12","10:35:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-62430",81906,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0684538,-112.1514958,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994245455","Not Detected","None","1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40316.CHEM/results/994245455/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-29T14:35:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48327.CHEM","Sample-Routine","Water","Groundwater","2021-11-17","09:55:00","MST",{"$nulls":4},67,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63181",82500,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7235,-112.0051,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993005456","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},67,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48327.CHEM/results/993005456/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2023-11-09T09:47:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44866.CHEM","Sample-Routine","Water","Groundwater","2021-06-01","03:07:00","MST",{"$nulls":4},118,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-40429",46747,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49439,-112.00447,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974183331","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},118,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44866.CHEM/results/974183331/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-05-05T10:01:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36458.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-11-10","03:17:00","MST",{"$nulls":4},118,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62928",82297,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.1818502,-110.9567339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937424019","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},118,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36458.CHEM/results/937424019/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:37:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33254.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","08:14:00","MST",{"$nulls":4},240,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916460215","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,D1,V1,L5.",null,240,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33254.CHEM/results/916460215/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2021-10-19T11:12:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33217.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","08:24:00","MST",{"$nulls":4},179,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-59185",80570,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3634244,-111.8141481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916462361","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,179,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33217.CHEM/results/916462361/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:13:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37392.CHEM","Sample-Routine","Water","Groundwater","2021-10-22","10:45:00","MST",{"$nulls":4},89,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58665",79061,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5095861,-112.0477528,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943310859","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},89,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37392.CHEM/results/943310859/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-07-05T13:16:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44913.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","11:37:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974186974","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44913.CHEM/results/974186974/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:07:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35005.CHEM","Sample-Routine","Water","Groundwater","2021-12-19","03:24:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52862",63334,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2014664,-110.9687608,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994628793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35005.CHEM/results/994628793/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:14:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35590.CHEM","Sample-Routine","Water","Groundwater","2021-09-23","10:40:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63056",82390,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484119,-112.1499339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933548167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35590.CHEM/results/933548167/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-03-25T10:45:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33060.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","10:24:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62544",81979,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934,-111.9863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916455110","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33060.CHEM/results/916455110/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35195.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","02:01:00","MST",{"$nulls":4},27,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62380",81862,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2204781,-114.564655,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994629716","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,27,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35195.CHEM/results/994629716/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:14:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47791.CHEM","Sample-Routine","Water","Groundwater","2021-10-20","10:10:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62533",81970,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5257523,-112.0817348,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-979418815","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47791.CHEM/results/979418815/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-06-26T10:50:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34005.CHEM","Sample-Routine","Water","Groundwater","2021-09-30","03:38:00","MST",{"$nulls":4},72.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62900",82271,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4806301,-112.0127084,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919350985","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,72.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34005.CHEM/results/919350985/resdetectqntlmts","Laboratory Reporting Level",640,"ug/L",null,"2021-11-23T10:08:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36454.CHEM","Sample-Routine","Water","Groundwater","2021-11-10","08:28:00","MST",{"$nulls":4},116,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62930",82299,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.1814244,-110.9569645,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937423723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},116,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36454.CHEM/results/937423723/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:37:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36419.CHEM","Sample-Routine","Water","Groundwater","2021-12-15","03:03:00","MST",{"$nulls":4},99,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62945",82311,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.383618,-110.7758978,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937420901","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,99,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36419.CHEM/results/937420901/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:36:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36446.CHEM","Sample-Routine","Water","Groundwater","2021-11-09","11:10:00","MST",{"$nulls":4},118,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62926",82295,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.1817112,-110.9566139,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937423131","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},118,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36446.CHEM/results/937423131/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:36:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35335.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-08","12:00:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62990",82356,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3352725,-110.9420124,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994634659","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35335.CHEM/results/994634659/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:15:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34994.CHEM","Sample-Routine","Water","Groundwater","2021-11-29","02:20:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62648",82055,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0190483,-110.6830206,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994138716","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34994.CHEM/results/994138716/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",null,"2023-11-29T09:07:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34787.CHEM","Sample-Routine","Water","Groundwater","2021-11-19","02:45:00","MST",{"$nulls":11},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62552",81987,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.901399,-110.159333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992883677","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34787.CHEM/results/992883677/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:35:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33077.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","09:58:00","MST",{"$nulls":4},240,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50243",60346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3780192,-111.8242253,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916457107","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,240,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33077.CHEM/results/916457107/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33045.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","08:36:00","MST",{"$nulls":4},44,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-55856",69398,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4952683,-111.9801764,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916453852","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,44,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33045.CHEM/results/916453852/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36413.CHEM","Sample-Routine","Water","Groundwater","2021-12-17","08:17:00","MST",{"$nulls":4},81,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62942",82308,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833726,-110.7762585,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937420331","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,81,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36413.CHEM/results/937420331/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:36:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35579.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","02:52:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63066",82400,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481667,-112.1489083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933547342","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35579.CHEM/results/933547342/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",null,"2022-03-25T10:44:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34199.CHEM","Sample-Routine","Water","Groundwater","2021-11-17","10:07:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-61927",81615,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2011667,-110.9686,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-925214194","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34199.CHEM/results/925214194/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2021-12-28T10:27:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48324.CHEM","Sample-Routine","Water","Groundwater","2021-11-17","10:15:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63183",82502,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.723368,-112.004736,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993005233","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48324.CHEM/results/993005233/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2023-11-09T09:47:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33356.CHEM","Sample-Routine","Water","Groundwater","2021-09-01","10:50:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62667",82072,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2566243,-114.1468746,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916470597","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33356.CHEM/results/916470597/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:15:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44703.CHEM","Sample-Routine","Water","Groundwater","2022-09-29","09:55:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63533",82845,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9150811,-110.1535198,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994693931","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44703.CHEM/results/994693931/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:20:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49848.CHEM","Sample-Routine","Water","Groundwater","2022-02-18","10:25:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62521",81958,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.525761,-112.081087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999764445","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49848.CHEM/results/999764445/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2024-01-19T08:41:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48372.CHEM","Sample-Routine","Water","Groundwater","2022-02-09","02:43:00","MST",{"$nulls":4},153,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62063",81673,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6936881,-114.6224007,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993006037","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},153,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48372.CHEM/results/993006037/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48013.CHEM","Sample-Routine","Water","Groundwater","2022-10-04","07:00:00","MST",{"$nulls":4},190,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59223",80866,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5275649,-112.0813322,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992994142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},190,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48013.CHEM/results/992994142/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:46:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43315.CHEM","Sample-Routine","Water","Groundwater","2022-05-17","10:37:00","MST",{"$nulls":4},260,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62809",82188,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5123828,-112.1735089,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992935974","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},260,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43315.CHEM/results/992935974/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41272.CHEM","Sample-Routine","Water","Groundwater","2022-10-06","12:25:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63001",82366,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.5067521,-109.3643126,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-958332709","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41272.CHEM/results/958332709/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-11-29T09:04:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40418.CHEM","Sample-Routine","Water","Groundwater","2022-01-17","01:15:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-62433",81909,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0676359,-112.1512798,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999447150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40418.CHEM/results/999447150/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-16T10:10:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39782.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","01:27:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918478","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39782.CHEM/results/992918478/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48453.CHEM","Sample-Routine","Water","Groundwater","2022-02-22","11:05:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62161",81716,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5249138,-112.0816383,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993002978","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48453.CHEM/results/993002978/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36660.CHEM","Sample-Routine","Water","Groundwater","2022-04-12","06:04:00","MST",{"$nulls":4},27,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49222",59152,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2213989,-114.5633969,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994647681","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,27,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36660.CHEM/results/994647681/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37043.CHEM","Sample-Routine","Water","Groundwater","2022-05-12","01:15:00","MST",{"$nulls":4},23,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63070",82404,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0478107,-112.1488738,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650331","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,23,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37043.CHEM/results/994650331/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39010.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-06-17","12:14:00","MST",{"$nulls":4},213,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62912",82282,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387948,-112.1870131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953579031","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},213,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39010.CHEM/results/953579031/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-10-07T10:33:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43181.CHEM","Sample-Routine","Water","Groundwater","2022-11-08","02:08:00","MST",{"$nulls":4},16,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47012",56624,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0477975,-112.1493457,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994682833","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,16,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43181.CHEM/results/994682833/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:19:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41691.CHEM","Sample-Routine","Water","Groundwater","2022-11-14","02:56:00","MST",{"$nulls":4},10,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62662",82069,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0188803,-110.6848324,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679733","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,10,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41691.CHEM/results/994679733/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:19:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48461.CHEM","Sample-Routine","Water","Groundwater","2022-02-22","10:55:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62162",81717,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5249151,-112.0816389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993004162","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48461.CHEM/results/993004162/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41591.CHEM","Sample-Routine","Water","Groundwater","2022-12-08","12:38:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63002",82367,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.5067666,-109.3642005,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969239481","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41591.CHEM/results/969239481/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-03-03T09:05:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37445.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","05:50:00","MST",{"$nulls":4},350,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62804",82183,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5147024,-112.0742958,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},350,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37445.CHEM/results/992900729/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45352.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","11:15:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47087",56706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4263119,-111.9909864,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992975214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45352.CHEM/results/992975214/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41702.CHEM","Sample-Routine","Water","Groundwater","2022-11-17","01:30:00","MST",{"$nulls":4},12,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62652",82059,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0193513,-110.6837152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994680755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,12,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41702.CHEM/results/994680755/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",null,"2023-12-04T10:19:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36524.CHEM","Sample-Routine","Water","Groundwater","2022-03-11","09:52:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63014",82378,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.879284,-111.7359009,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994645531","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36524.CHEM/results/994645531/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:16:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43662.CHEM","Sample-Routine","Water","Groundwater","2022-04-27","10:48:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992945002","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43662.CHEM/results/992945002/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45266.CHEM","Sample-Routine","Water","Groundwater","2022-11-14","12:05:00","MST",{"$nulls":4},253,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62813",82192,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5073158,-112.16763,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992973808","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},253,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45266.CHEM/results/992973808/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39008.CHEM","Sample-Routine","Water","Groundwater","2022-06-16","10:59:00","MST",{"$nulls":4},217,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62914",82284,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5388505,-112.1868884,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953578883","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},217,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39008.CHEM/results/953578883/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-10-07T10:33:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41371.CHEM","Sample-Routine","Water","Groundwater","2022-11-11","10:20:00","MST",{"$nulls":4},217,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62915",82285,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387092,-112.1870093,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969238126","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},217,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41371.CHEM/results/969238126/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-03-03T09:05:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38455.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-06-09","12:30:00","MST",{"$nulls":4},48,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63126",82446,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7401428,-112.0096772,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943319977","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},48,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38455.CHEM/results/943319977/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-07-05T13:20:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41526.CHEM","Sample-Routine","Water","Groundwater","2022-11-23","01:34:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52698",63128,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016983,-110.9688897,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994676743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41526.CHEM/results/994676743/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:19:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48763.CHEM","Sample-Routine","Water","Groundwater","2022-11-10","10:10:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63557",82864,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.499442,-112.1447939,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993028645","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48763.CHEM/results/993028645/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:49:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39298.CHEM","Sample-Routine","Water","Groundwater","2022-08-27","01:47:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62743",82131,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0191229,-110.6824885,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994660668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39298.CHEM/results/994660668/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:17:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41677.CHEM","Sample-Routine","Water","Groundwater","2022-11-22","04:43:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62969",82335,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7310861,-111.9967444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992922788","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41677.CHEM/results/992922788/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39766.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","01:55:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917390","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39766.CHEM/results/992917390/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41213.CHEM","Sample-Routine","Water","Groundwater","2022-09-22","09:57:00","MST",{"$nulls":4},29.3,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62990",82356,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3352725,-110.9420124,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994673380","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,29.3,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41213.CHEM/results/994673380/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:18:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38961.CHEM","Sample-Routine","Water","Groundwater","2022-04-01","08:10:00","MST",{"$nulls":4},69,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62938",82304,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833563,-110.7760749,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-950633775","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},69,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38961.CHEM/results/950633775/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-08-30T11:00:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43341.CHEM","Sample-Routine","Water","Groundwater","2022-05-18","11:57:00","MST",{"$nulls":4},255,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63275",82593,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.499151,-112.1661915,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992937898","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},255,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43341.CHEM/results/992937898/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40577.CHEM","Sample-Routine","Water","Groundwater","2022-01-26","02:25:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63510",82822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2124908,-110.9688051,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999758296","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40577.CHEM/results/999758296/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-19T08:41:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45198.CHEM","Sample-Routine","Water","Groundwater","2022-10-17","11:40:00","MST",{"$nulls":4},155,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63289",82607,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4899618,-112.008548,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992970329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},155,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45198.CHEM/results/992970329/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48828.CHEM","Sample-Routine","Water","Groundwater","2022-08-29","01:00:00","MST",{"$nulls":4},145,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61895",81583,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6930367,-114.6198697,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993011327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},145,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48828.CHEM/results/993011327/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47512.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","01:00:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-49044",58917,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2445478,-111.3361836,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986968","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47512.CHEM/results/992986968/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39530.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","12:15:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992916981","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39530.CHEM/results/992916981/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:38:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41252.CHEM","Sample-Routine","Water","Groundwater","2022-06-02","10:45:00","MST",{"$nulls":4},35,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62989",82355,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359302,-110.9417269,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994674583","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},35,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41252.CHEM/results/994674583/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",null,"2023-12-04T10:19:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42935.CHEM","Sample-Routine","Water","Groundwater","2022-06-21","09:09:00","MST",{"$nulls":4},413,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-46020",51324,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4736978,-111.7336331,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992928969","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,413,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42935.CHEM/results/992928969/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47533.CHEM","Sample-Routine","Water","Groundwater","2022-05-04","02:45:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-47577",57229,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.500345,-112.1462644,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992988452","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47533.CHEM/results/992988452/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:46:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43524.CHEM","Sample-Routine","Water","Groundwater","2022-08-09","02:26:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62691",82096,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4910788,-114.3469286,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992940858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43524.CHEM/results/992940858/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42948.CHEM","Sample-Routine","Water","Groundwater","2022-06-22","10:51:00","MST",{"$nulls":4},193,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63505",82817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4846778,-111.7287332,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992930098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,193,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42948.CHEM/results/992930098/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47560.CHEM","Sample-Routine","Water","Groundwater","2022-04-29","07:50:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-56710",72021,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4990419,-112.1439442,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992988230","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47560.CHEM/results/992988230/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:46:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37042.CHEM","Sample-Routine","Water","Groundwater","2022-05-11","08:59:00","MST",{"$nulls":4},16,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47012",56624,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0477975,-112.1493457,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650254","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,16,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37042.CHEM/results/994650254/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45211.CHEM","Sample-Routine","Water","Groundwater","2022-10-18","09:35:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992971218","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45211.CHEM/results/992971218/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45230.CHEM","Sample-Routine","Water","Groundwater","2022-10-19","12:38:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992972624","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45230.CHEM/results/992972624/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39273.CHEM","Sample-Routine","Water","Groundwater","2022-08-26","06:32:00","MST",{"$nulls":4},212,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62915",82285,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387092,-112.1870093,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-951709035","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},212,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39273.CHEM/results/951709035/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",null,"2022-09-23T23:34:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48010.CHEM","Sample-Routine","Water","Groundwater","2022-10-03","12:50:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62530",81967,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5257528,-112.0818085,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992993920","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48010.CHEM/results/992993920/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2023-11-09T09:46:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43539.CHEM","Sample-Routine","Water","Groundwater","2022-08-08","02:42:00","MST",{"$nulls":4},245,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63302",82620,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.492867,-114.3461749,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992941968","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,245,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43539.CHEM/results/992941968/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40265.CHEM","Sample-Routine","Water","Groundwater","2022-09-22","09:23:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62777",82156,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2127512,-112.7555304,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956947825","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40265.CHEM/results/956947825/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2022-10-28T11:00:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36046.CHEM","Sample-Routine","Water","Groundwater","2022-03-03","01:22:00","MST",{"$nulls":4},16,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47011",56623,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482379,-112.1500859,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994643633","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},16,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36046.CHEM/results/994643633/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2023-12-04T10:16:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39545.CHEM","Sample-Routine","Water","Groundwater","2022-09-08","09:35:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-40431",46749,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4945336,-111.9822153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992913195","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8,V1,L5.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39545.CHEM/results/992913195/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:38:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49203.CHEM","Sample-Routine","Water","Groundwater","2022-10-12","12:47:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50273",60376,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5085703,-112.0739794,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993021612","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49203.CHEM/results/993021612/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:49:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36650.CHEM","Sample-Routine","Water","Groundwater","2022-04-15","08:35:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62375",81857,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2207392,-114.5638244,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994646873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36650.CHEM/results/994646873/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40670.CHEM","Sample-Routine","Water","Groundwater","2022-05-09","03:13:00","MST",{"$nulls":4},39,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63537",82849,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9150298,-110.1540659,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994668504","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},39,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40670.CHEM/results/994668504/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:18:34","STORET"]
["AZDEQ_GW","AZDEQ_GW","AZDEQ_GW-AB49487.CHEM","Sample-Routine","Water","Groundwater","2022-10-14","02:50:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9876,"2023_WQARF","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_GW-56546",71389,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4933,-112.0152528,"Unknown","AZDEQ_GW","Unknown",null,"Miscellaneous (Other)","STORET-999445171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_GW","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_GW/activities/AZDEQ_GW-AB49487.CHEM/results/999445171/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-16T10:09:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45207.CHEM","Sample-Routine","Water","Groundwater","2022-10-18","12:07:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63582",82873,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4914947,-112.0116,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992970922","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45207.CHEM/results/992970922/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39694.CHEM","Sample-Routine","Other","Groundwater","2022-04-21","03:22:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-954060018","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39694.CHEM/results/954060018/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2022-10-14T11:12:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40580.CHEM","Sample-Routine","Water","Groundwater","2022-01-26","09:40:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63520",82832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2126908,-110.9692678,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999758530","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40580.CHEM/results/999758530/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-19T08:41:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37388.CHEM","Sample-Routine","Water","Groundwater","2022-04-12","09:03:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992899839","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37388.CHEM/results/992899839/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:36:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48461.CHEM","Sample-Routine","Water","Groundwater","2022-02-22","10:55:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62162",81717,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5249151,-112.0816389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993004161","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48461.CHEM/results/993004161/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39186.CHEM","Sample-Routine","Water","Groundwater","2022-08-18","01:50:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-55718",69006,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.735,-112.0030556,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908372","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39186.CHEM/results/992908372/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38297.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-02","03:32:00","MST",{"$nulls":4},216,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62915",82285,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387092,-112.1870093,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943318789","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},216,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38297.CHEM/results/943318789/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-07-05T13:20:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43525.CHEM","Sample-Routine","Water","Groundwater","2022-08-09","12:00:00","MST",{"$nulls":4},187,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62814",82193,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4937948,-114.3462755,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992940932","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,187,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43525.CHEM/results/992940932/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36224.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","08:20:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62372",81854,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2200114,-114.5652772,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994644410","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,15,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36224.CHEM/results/994644410/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43034.CHEM","Sample-Routine","Water","Groundwater","2022-11-07","01:19:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-61668",81408,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2384587,-110.9754994,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992932348","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43034.CHEM/results/992932348/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39332.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","11:45:00","MST",{"$nulls":4},209.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62826",82204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651708,-112.4536862,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994661994","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,209.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39332.CHEM/results/994661994/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:17:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43104.CHEM","Sample-Routine","Water","Groundwater","2022-09-15","07:13:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","WSP USA ENVIRONMENT & INFRASTRUCTURE INC","AZDEQ_WPD-59185",80570,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3634244,-111.8141481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992935307","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43104.CHEM/results/992935307/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:40:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38750.CHEM","Sample-Routine","Water","Groundwater","2022-07-20","10:06:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50535",60650,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2257778,-110.8338333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992906743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38750.CHEM/results/992906743/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:37:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36232.CHEM","Sample-Routine","Water","Groundwater","2022-03-15","01:10:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62376",81858,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2207364,-114.5643189,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994645058","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36232.CHEM/results/994645058/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39690.CHEM","Sample-Routine","Other","Groundwater","2022-04-21","05:41:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-954059742","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39690.CHEM/results/954059742/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2022-10-14T11:12:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41636.CHEM","Sample-Routine","Water","Groundwater","2022-11-29","10:37:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62950",82316,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3835552,-110.7754037,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962655439","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41636.CHEM/results/962655439/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-01-06T10:31:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48830.CHEM","Sample-Routine","Water","Groundwater","2022-08-30","04:50:00","MST",{"$nulls":4},148,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61904",81592,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6940346,-114.6214261,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993011475","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},148,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48830.CHEM/results/993011475/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",null,"2023-11-09T09:48:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41632.CHEM","Sample-Routine","Water","Groundwater","2022-11-30","11:02:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62948",82314,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3835112,-110.7761864,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962655107","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41632.CHEM/results/962655107/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-01-06T10:31:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41167.CHEM","Sample-Routine","Water","Groundwater","2022-09-07","10:02:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47007",56619,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484,-112.148911,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994669939","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41167.CHEM/results/994669939/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:18:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39790.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","12:33:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992919022","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39790.CHEM/results/992919022/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42947.CHEM","Sample-Routine","Water","Groundwater","2022-06-21","10:32:00","MST",{"$nulls":4},412,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-46018",51322,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4720542,-111.7289603,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992930022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,412,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42947.CHEM/results/992930022/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39242.CHEM","Sample-Routine","Water","Groundwater","2022-08-27","05:58:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52798",63336,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018136,-110.9687664,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994659549","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39242.CHEM/results/994659549/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:17:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45228.CHEM","Sample-Routine","Water","Groundwater","2022-10-18","08:35:00","MST",{"$nulls":4},117,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54635",62158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.00218,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992972476","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},117,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45228.CHEM/results/992972476/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45203.CHEM","Sample-Routine","Water","Groundwater","2022-10-17","02:44:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63285",82603,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934158,-112.0072961,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992970699","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45203.CHEM/results/992970699/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45179.CHEM","Sample-Routine","Water","Groundwater","2022-10-19","12:24:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992968924","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45179.CHEM/results/992968924/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:43:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40268.CHEM","Sample-Routine","Water","Groundwater","2022-09-22","09:00:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62545",81980,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2121013,-112.7553064,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956948101","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40268.CHEM/results/956948101/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-10-28T11:00:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43338.CHEM","Sample-Routine","Water","Groundwater","2022-05-19","09:46:00","MST",{"$nulls":4},245,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63279",82597,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5139172,-112.1594514,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992937676","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},245,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43338.CHEM/results/992937676/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43125.CHEM","Sample-Routine","Water","Groundwater","2022-12-15","05:05:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63531",82843,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.915086,-110.1538981,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994687258","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43125.CHEM/results/994687258/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",null,"2023-12-04T10:20:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37068.CHEM","Sample-Routine","Water","Groundwater","2022-05-11","11:19:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62779",82158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.212335,-112.7553257,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994651283","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37068.CHEM/results/994651283/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:17:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39789.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","11:38:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918954","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39789.CHEM/results/992918954/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44706.CHEM","Sample-Routine","Water","Groundwater","2022-09-29","04:10:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63532",82844,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9153846,-110.1540088,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994693851","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44706.CHEM/results/994693851/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:20:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41249.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-06-02","12:00:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62983",82349,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357611,-110.9416976,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994674358","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41249.CHEM/results/994674358/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:19:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41259.CHEM","Sample-Routine","Water","Groundwater","2022-06-01","08:36:00","MST",{"$nulls":4},46,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62985",82351,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359064,-110.9418538,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994675123","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},46,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41259.CHEM/results/994675123/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:19:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42923.CHEM","Sample-Routine","Water","Groundwater","2022-06-15","01:47:00","MST",{"$nulls":4},240,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63496",82808,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4839139,-111.7258322,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992927840","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,240,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42923.CHEM/results/992927840/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35748.CHEM","Sample-Routine","Water","Groundwater","2022-02-18","06:14:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52799",63337,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2019433,-110.9690472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994637058","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35748.CHEM/results/994637058/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:15:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43124.CHEM","Sample-Routine","Water","Groundwater","2022-12-15","04:00:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63534",82846,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152395,-110.1541575,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994687177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43124.CHEM/results/994687177/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2023-12-04T10:20:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49863.CHEM","Sample-Routine","Water","Groundwater","2022-02-17","11:45:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63168",82487,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5275367,-112.0809018,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999765341","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49863.CHEM/results/999765341/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2024-01-19T08:41:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39785.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","02:49:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918682","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39785.CHEM/results/992918682/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37535.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","10:22:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50534",60649,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2331389,-110.84327,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992904280","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,H1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37535.CHEM/results/992904280/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:37:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39179.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","02:15:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62687",82092,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7296278,-112.0082889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992907854","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39179.CHEM/results/992907854/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48811.CHEM","Sample-Routine","Water","Groundwater","2022-08-29","10:00:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61895",81583,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6930367,-114.6198697,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993010125","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48811.CHEM/results/993010125/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37447.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","08:58:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62802",82181,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5086378,-112.0724669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900877","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37447.CHEM/results/992900877/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43094.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","12:02:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62133",81708,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271694,-110.8374424,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992934567","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43094.CHEM/results/992934567/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:40:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41687.CHEM","Sample-Routine","Water","Groundwater","2022-11-15","01:00:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62646",82053,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184087,-110.6844699,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679363","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41687.CHEM/results/994679363/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-12-04T10:19:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39204.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","11:00:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-55710",68998,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7216667,-111.9961111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992909704","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39204.CHEM/results/992909704/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40666.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","03:18:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63530",82842,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152019,-110.1540564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994668204","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40666.CHEM/results/994668204/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2023-12-04T10:18:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41637.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-11-30","03:39:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62940",82306,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834931,-110.7759672,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962655530","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41637.CHEM/results/962655530/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-01-06T10:31:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43092.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","11:35:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-47634",57289,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271944,-110.8376042,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992934419","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43092.CHEM/results/992934419/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:39:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48419.CHEM","Sample-Routine","Water","Groundwater","2022-02-09","03:30:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62273",81774,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6946679,-114.6225119,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993007449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48419.CHEM/results/993007449/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48191.CHEM","Sample-Routine","Water","Groundwater","2023-01-31","09:10:00","MST",{"$nulls":4},136,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62275",81776,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6930332,-114.6196025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999654839","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},136,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48191.CHEM/results/999654839/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2024-01-18T09:31:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45339.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","09:10:00","MST",{"$nulls":4},37.8,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63099",82425,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.286038,-110.1182718,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974804165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},37.8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45339.CHEM/results/974804165/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-05-23T13:51:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43977.CHEM","Sample-Routine","Other","Groundwater","2023-02-08","03:33:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62550",81985,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006402,-110.159209,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992955220","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43977.CHEM/results/992955220/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48186.CHEM","Sample-Routine","Water","Groundwater","2023-01-30","01:55:00","MST",{"$nulls":4},185,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62072",81682,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.693765,-114.6214204,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999654610","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},185,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48186.CHEM/results/999654610/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2024-01-18T09:31:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45513.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","09:18:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62986",82352,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357379,-110.9421479,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994696125","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,36,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45513.CHEM/results/994696125/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:20:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45169.CHEM","Sample-Routine","Water","Groundwater","2023-03-24","09:47:00","MST",{"$nulls":4},38,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62869",82240,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530225,-110.0338642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974992693","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,38,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45169.CHEM/results/974992693/resdetectqntlmts","Laboratory Reporting Level",160,"ug/L",null,"2023-05-25T10:52:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48995.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-03-28","03:30:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993017912","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48995.CHEM/results/993017912/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45496.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","09:34:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62974",82340,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357648,-110.9417321,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994694854","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45496.CHEM/results/994694854/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:20:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47278.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","10:40:00","MST",{"$nulls":4},128,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63203",82522,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6955101,-114.6203574,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999651706","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},128,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47278.CHEM/results/999651706/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-18T09:30:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45641.CHEM","Sample-Routine","Water","Groundwater","2023-03-30","08:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59329",81031,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2290775,-111.3276856,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992977697","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45641.CHEM/results/992977697/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47277.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","01:05:00","MST",{"$nulls":4},140,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62059",81669,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6941941,-114.6203401,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999215611","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},140,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47277.CHEM/results/999215611/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-09T09:21:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49471.CHEM","Sample-Routine","Water","Groundwater","2023-03-30","01:30:00","MST",{"$nulls":4},230,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48036",57704,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2285256,-111.3335314,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999763389","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},230,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49471.CHEM/results/999763389/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-19T08:41:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48074.CHEM","Sample-Routine","Water","Groundwater","2023-01-25","02:30:00","MST",{"$nulls":4},128,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63203",82522,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6955101,-114.6203574,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999654154","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},128,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48074.CHEM/results/999654154/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-18T09:30:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44371.CHEM","Sample-Routine","Other","Groundwater","2023-02-09","01:54:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992961989","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44371.CHEM/results/992961989/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:43:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43975.CHEM","Sample-Routine","Other","Groundwater","2023-02-08","03:49:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992955084","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43975.CHEM/results/992955084/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46331.CHEM","Sample-Routine","Water","Groundwater","2023-03-16","12:35:00","MST",{"$nulls":4},102.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63023",82387,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.879323,-111.7356152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994697697","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,102.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46331.CHEM/results/994697697/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49080.CHEM","Sample-Routine","Water","Groundwater","2023-05-31","12:25:00","MST",{"$nulls":4},102.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63082",82408,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8794124,-111.7349297,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704403","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,102.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49080.CHEM/results/994704403/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49083.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","01:40:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62987",82353,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3360385,-110.9420765,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49083.CHEM/results/994704632/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46601.CHEM","Sample-Routine","Other","Groundwater","2023-05-10","10:09:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992984000","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46601.CHEM/results/992984000/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:45:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49091.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","08:37:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62981",82347,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356215,-110.9418144,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705226","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49091.CHEM/results/994705226/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46311.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","09:30:00","MST",{"$nulls":4},142,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55380",68281,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6932833,-114.6211361,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992979334","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},142,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46311.CHEM/results/992979334/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",null,"2023-11-09T09:45:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49164.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","11:26:00","MST",{"$nulls":4},58,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59152",80430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1514111,-109.9719722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016802","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},58,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49164.CHEM/results/993016802/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49137.CHEM","Sample-Routine","Water","Groundwater","2023-04-18","01:17:00","MST",{"$nulls":4},89,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58665",79061,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5095861,-112.0477528,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016062","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,89,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49137.CHEM/results/993016062/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46587.CHEM","Sample-Routine","Other","Groundwater","2023-05-10","02:49:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992983048","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46587.CHEM/results/992983048/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:45:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49081.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","09:25:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63016",82380,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8793638,-111.7360725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704477","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49081.CHEM/results/994704477/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46602.CHEM","Sample-Routine","Other","Groundwater","2023-05-10","09:09:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992984068","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46602.CHEM/results/992984068/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:45:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49096.CHEM","Sample-Routine","Water","Groundwater","2023-06-08","08:34:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62988",82354,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.33581,-110.9417227,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705598","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49096.CHEM/results/994705598/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49097.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-07","04:26:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62989",82355,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359302,-110.9417269,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705672","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49097.CHEM/results/994705672/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50499.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","09:55:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63055",82389,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0487386,-112.1489839,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706269","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50499.CHEM/results/994706269/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46358.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","02:34:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62951",82317,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833447,-110.7755438,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983663076","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46358.CHEM/results/983663076/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-07-26T11:00:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46594.CHEM","Sample-Routine","Other","Groundwater","2023-05-10","10:56:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992983524","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46594.CHEM/results/992983524/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:45:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46344.CHEM","Sample-Routine","Water","Groundwater","2023-04-27","11:10:00","MST",{"$nulls":4},84,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: M1,R5,.",null,84,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46344.CHEM/results/983662034/resdetectqntlmts","Laboratory Reporting Level",5.98,"ug/L",null,"2023-07-26T11:00:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46347.CHEM","Sample-Routine","Water","Groundwater","2023-04-26","12:38:00","MST",{"$nulls":4},74,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62938",82304,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833563,-110.7760749,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662257","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},74,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46347.CHEM/results/983662257/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-07-26T11:00:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48571.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","01:45:00","MST",{"$nulls":4},159,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-15970",24732,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6941992,-114.6281436,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993001343","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,159,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48571.CHEM/results/993001343/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:47:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49158.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","02:17:00","MST",{"$nulls":4},65,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016358","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},65,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49158.CHEM/results/993016358/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49161.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","12:47:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016580","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49161.CHEM/results/993016580/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46577.CHEM","Sample-Routine","Other","Groundwater","2023-05-11","04:45:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992982368","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46577.CHEM/results/992982368/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:45:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46222.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:20:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-54199",65608,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5280103,-112.0834631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992985027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46222.CHEM/results/992985027/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:45:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49085.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","10:35:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62978",82344,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358918,-110.9416598,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49085.CHEM/results/994704780/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45529.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:14:00","MST",{"$nulls":4},30.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62862",82233,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.255957,-110.0239318,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083461","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,30.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45529.CHEM/results/975083461/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-05-30T10:53:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49086.CHEM","Sample-Routine","Water","Groundwater","2023-06-08","11:50:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62979",82345,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357929,-110.9418056,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704854","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49086.CHEM/results/994704854/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48987.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","12:37:00","MST",{"$nulls":4},305,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62775",82154,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4867908,-112.100564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013990","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},305,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48987.CHEM/results/993013990/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50498.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","11:01:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47007",56619,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484,-112.148911,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706195","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50498.CHEM/results/994706195/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46345.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","12:56:00","MST",{"$nulls":4},96,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62945",82311,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.383618,-110.7758978,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},96,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46345.CHEM/results/983662109/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-07-26T11:00:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50501.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","03:34:00","MST",{"$nulls":4},6,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63056",82390,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484119,-112.1499339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706421","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50501.CHEM/results/994706421/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48546.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","10:55:00","MST",{"$nulls":4},165,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61907",81595,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6943898,-114.6224328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999760256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,165,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48546.CHEM/results/999760256/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-19T08:41:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50510.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","08:45:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47010",56622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048881,-112.1491475,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994707096","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50510.CHEM/results/994707096/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50506.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-02","11:37:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63061",82395,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483203,-112.1490083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706798","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,H1,.",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50506.CHEM/results/994706798/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46309.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","10:55:00","MST",{"$nulls":4},195,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55494",68499,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945844,-114.6232625,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992979185","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},195,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46309.CHEM/results/992979185/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:45:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46310.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","10:05:00","MST",{"$nulls":4},136,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62057",81667,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6938676,-114.6203393,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999651493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,136,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46310.CHEM/results/999651493/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2024-01-18T09:30:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49098.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-07","09:35:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62983",82349,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357611,-110.9416976,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705747","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49098.CHEM/results/994705747/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48983.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","11:04:00","MST",{"$nulls":4},134,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62774",82153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4868778,-112.1006288,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013694","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},134,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48983.CHEM/results/993013694/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49087.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","03:25:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49087.CHEM/results/994704928/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",null,"2023-12-04T10:21:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46352.CHEM","Sample-Routine","Water","Groundwater","2023-04-26","10:48:00","MST",{"$nulls":4},103,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62941",82307,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3840379,-110.7762873,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},103,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46352.CHEM/results/983662632/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-07-26T11:00:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49082.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","02:56:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62985",82351,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359064,-110.9418538,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704551","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49082.CHEM/results/994704551/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48988.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","11:25:00","MST",{"$nulls":4},141,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62774",82153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4868778,-112.1006288,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993014064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},141,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48988.CHEM/results/993014064/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49092.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","04:15:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62984",82350,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358115,-110.9418872,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705300","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49092.CHEM/results/994705300/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48552.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","10:20:00","MST",{"$nulls":4},147,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61904",81592,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6940346,-114.6214261,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992999924","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},147,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48552.CHEM/results/992999924/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:47:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46604.CHEM","Sample-Routine","Other","Groundwater","2023-05-11","02:25:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992984204","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46604.CHEM/results/992984204/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:45:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48982.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-04-14","12:00:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62776",82155,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.485781,-112.1016998,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013620","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48982.CHEM/results/993013620/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48558.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","09:50:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62060",81670,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6933939,-114.6214188,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993000372","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48558.CHEM/results/993000372/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:47:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49167.CHEM","Sample-Routine","Water","Groundwater","2023-04-05","12:05:00","MST",{"$nulls":4},155,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993017024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},155,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49167.CHEM/results/993017024/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45531.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","02:34:00","MST",{"$nulls":4},28,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62859",82230,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2558122,-110.0239078,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083571","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,28,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45531.CHEM/results/975083571/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-05-30T10:53:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50985.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","12:41:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035265","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50985.CHEM/results/993035265/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51525.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","11:17:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52476",62766,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2259808,-110.9666858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038566","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51525.CHEM/results/993038566/resdetectqntlmts","Laboratory Reporting Level",0.0443,"mg/m3",null,"2023-11-09T09:50:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50984.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","09:31:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035197","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50984.CHEM/results/993035197/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51002.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:55:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036421","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51002.CHEM/results/993036421/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50996.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","12:05:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036013","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50996.CHEM/results/993036013/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50980.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","08:33:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034925","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50980.CHEM/results/993034925/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50893.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","10:36:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63479",82795,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9009139,-110.1588167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034449","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50893.CHEM/results/993034449/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50992.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","04:09:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035741","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50992.CHEM/results/993035741/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51533.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","01:10:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52475",62765,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258156,-110.9669394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993039110","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51533.CHEM/results/993039110/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51531.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","09:28:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63545",82856,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2259876,-110.9667495,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038974","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},45,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51531.CHEM/results/993038974/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50993.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","10:42:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62324",81825,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035809","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50993.CHEM/results/993035809/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50888.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","02:59:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034109","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50888.CHEM/results/993034109/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50988.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","12:43:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62338",81835,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035469","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50988.CHEM/results/993035469/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50983.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:01:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62333",81830,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035129","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50983.CHEM/results/993035129/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50987.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","10:51:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62322",81823,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035401","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50987.CHEM/results/993035401/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50986.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:44:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035333","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50986.CHEM/results/993035333/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50978.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","11:45:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034789","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50978.CHEM/results/993034789/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50974.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","03:33:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62314",81815,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034517","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50974.CHEM/results/993034517/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50982.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:57:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62340",81837,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035061","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50982.CHEM/results/993035061/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50995.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:57:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035945","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50995.CHEM/results/993035945/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51004.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","04:25:00","MST",{"$nulls":4},13.7,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62317",81818,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036557","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},13.7,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51004.CHEM/results/993036557/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50889.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","01:43:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63480",82796,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9007889,-110.1590667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034177","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50889.CHEM/results/993034177/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51529.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","12:21:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63546",82857,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258496,-110.9666718,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038838","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51529.CHEM/results/993038838/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51001.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","10:46:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036353","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51001.CHEM/results/993036353/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51527.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","03:35:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52474",62764,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258108,-110.9664744,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038702","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51527.CHEM/results/993038702/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50981.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","02:33:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034993","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50981.CHEM/results/993034993/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50998.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:14:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036149","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50998.CHEM/results/993036149/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50994.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","02:13:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035877","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50994.CHEM/results/993035877/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50976.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","12:10:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62337",81834,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034653","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50976.CHEM/results/993034653/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50891.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","02:38:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034313","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50891.CHEM/results/993034313/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51528.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:38:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63547",82858,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2260778,-110.9664476,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038770","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51528.CHEM/results/993038770/resdetectqntlmts","Laboratory Reporting Level",0.0443,"mg/m3",null,"2023-11-09T09:50:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51530.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:57:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63544",82855,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258612,-110.9668172,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038906","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51530.CHEM/results/993038906/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50989.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:42:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035537","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50989.CHEM/results/993035537/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50890.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","04:23:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034245","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50890.CHEM/results/993034245/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50991.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:32:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035673","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50991.CHEM/results/993035673/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51005.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","12:20:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036625","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51005.CHEM/results/993036625/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51526.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","01:24:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52473",62763,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2262686,-110.9664731,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038634","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51526.CHEM/results/993038634/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50997.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","10:13:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62311",81812,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232588,-110.972266,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036081","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50997.CHEM/results/993036081/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51532.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:18:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63543",82854,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2260615,-110.9666247,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993039042","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51532.CHEM/results/993039042/resdetectqntlmts","Laboratory Reporting Level",0.443,"mg/m3",null,"2023-11-09T09:50:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50979.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:03:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034857","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50979.CHEM/results/993034857/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50999.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","02:50:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036217","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50999.CHEM/results/993036217/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51003.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","11:24:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036489","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51003.CHEM/results/993036489/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50977.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","02:01:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62342",81839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034721","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50977.CHEM/results/993034721/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50975.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","03:49:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62315",81816,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034585","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50975.CHEM/results/993034585/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50892.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","03:35:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63478",82794,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9005639,-110.1590444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034381","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50892.CHEM/results/993034381/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50990.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","12:22:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62318",81819,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035605","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50990.CHEM/results/993035605/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51000.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:17:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036285","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51000.CHEM/results/993036285/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52416.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:03:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361574","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52416.CHEM/results/997361574/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52440.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","10:56:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363206","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52440.CHEM/results/997363206/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52430.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:10:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362526","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52430.CHEM/results/997362526/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52347.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","03:48:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323972","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52347.CHEM/results/997323972/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52415.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","01:36:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361506","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52415.CHEM/results/997361506/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52417.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:09:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62333",81830,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361642","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52417.CHEM/results/997361642/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52343.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","05:25:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63479",82795,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9009139,-110.1588167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323700","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52343.CHEM/results/997323700/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-28T09:24:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52345.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","03:14:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323836","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52345.CHEM/results/997323836/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52427.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:38:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62338",81835,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362322","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52427.CHEM/results/997362322/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52439.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:12:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363138","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52439.CHEM/results/997363138/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52432.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:36:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62318",81819,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362662","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52432.CHEM/results/997362662/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52433.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:24:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362730","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52433.CHEM/results/997362730/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52436.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:44:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62342",81839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362934","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52436.CHEM/results/997362934/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52344.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","04:51:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323768","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52344.CHEM/results/997323768/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-28T09:24:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52420.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:59:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361846","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52420.CHEM/results/997361846/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52434.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:46:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362798","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52434.CHEM/results/997362798/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52437.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:28:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62337",81834,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363002","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52437.CHEM/results/997363002/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52414.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:16:00","MST",{"$nulls":4},13.7,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62317",81818,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361438","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},13.7,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52414.CHEM/results/997361438/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52418.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:40:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62315",81816,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361710","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52418.CHEM/results/997361710/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52422.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:52:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361982","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52422.CHEM/results/997361982/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52426.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:54:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362254","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52426.CHEM/results/997362254/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52441.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:23:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62314",81815,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363274","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52441.CHEM/results/997363274/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52348.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","02:48:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63480",82796,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9007889,-110.1590667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997324040","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52348.CHEM/results/997324040/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-28T09:24:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52429.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","10:49:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362458","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52429.CHEM/results/997362458/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52435.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","11:30:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62311",81812,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232588,-110.972266,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362866","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52435.CHEM/results/997362866/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52428.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","01:12:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362390","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52428.CHEM/results/997362390/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52425.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","10:30:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362186","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52425.CHEM/results/997362186/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52411.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","11:13:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361234","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52411.CHEM/results/997361234/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52412.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:03:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361302","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52412.CHEM/results/997361302/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52438.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:56:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62322",81823,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363070","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52438.CHEM/results/997363070/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52346.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","04:22:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63478",82794,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9005639,-110.1590444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323904","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52346.CHEM/results/997323904/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52442.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:31:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62340",81837,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363342","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52442.CHEM/results/997363342/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52424.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:01:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362118","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52424.CHEM/results/997362118/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52419.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:46:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361778","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52419.CHEM/results/997361778/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52413.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","10:50:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361370","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52413.CHEM/results/997361370/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52431.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","02:02:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362594","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52431.CHEM/results/997362594/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52421.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:08:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361914","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52421.CHEM/results/997361914/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52423.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","12:40:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62324",81825,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362050","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52423.CHEM/results/997362050/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:48","STORET"]

{"sheet":"Surface water","index":4,"n_rows":10210,"n_cols":83,"rows_kept":1125,"cut":true,"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
["OrganizationIdentifier","OrganizationFormalName","ActivityIdentifier","ActivityTypeCode","ActivityMediaName","ActivityMediaSubdivisionName","ActivityStartDate","ActivityStartTime/Time","ActivityStartTime/TimeZoneCode","ActivityEndDate","ActivityEndTime/Time","ActivityEndTime/TimeZoneCode","ActivityRelativeDepthName","ActivityDepthHeightMeasure/MeasureValue","ActivityDepthHeightMeasure/MeasureUnitCode","ActivityDepthAltitudeReferencePointText","ActivityTopDepthHeightMeasure/MeasureValue","ActivityTopDepthHeightMeasure/MeasureUnitCode","ActivityBottomDepthHeightMeasure/MeasureValue","ActivityBottomDepthHeightMeasure/MeasureUnitCode","ProjectIdentifier","ProjectName","ActivityConductingOrganizationText","MonitoringLocationIdentifier","MonitoringLocationName","ActivityCommentText","SampleAquifer","HydrologicCondition","HydrologicEvent","ActivityLocation/LatitudeMeasure","ActivityLocation/LongitudeMeasure","SampleCollectionMethod/MethodIdentifier","SampleCollectionMethod/MethodIdentifierContext","SampleCollectionMethod/MethodName","SampleCollectionMethod/MethodDescriptionText","SampleCollectionEquipmentName","ResultIdentifier","ResultDetectionConditionText","MethodSpeciationName","CharacteristicName","ResultSampleFractionText","ResultMeasureValue","ResultMeasure/MeasureUnitCode","MeasureQualifierCode","ResultStatusIdentifier","StatisticalBaseCode","ResultValueTypeName","ResultWeightBasisText","ResultTimeBasisText","ResultTemperatureBasisText","ResultParticleSizeBasisText","DataQuality/PrecisionValue","DataQuality/BiasValue","DataQuality/ConfidenceIntervalValue","DataQuality/UpperConfidenceLimitValue","DataQuality/LowerConfidenceLimitValue","ResultCommentText","USGSPCode","ResultDepthHeightMeasure/MeasureValue","ResultDepthHeightMeasure/MeasureUnitCode","ResultDepthAltitudeReferencePointText","SubjectTaxonomicName","SampleTissueAnatomyName","BinaryObjectFileName","BinaryObjectFileTypeCode","ResultFileUrl","ResultAnalyticalMethod/MethodIdentifier","ResultAnalyticalMethod/MethodIdentifierContext","ResultAnalyticalMethod/MethodName","ResultAnalyticalMethod/MethodUrl","ResultAnalyticalMethod/MethodDescriptionText","LaboratoryName","AnalysisStartDate","ResultLaboratoryCommentText","ResultDetectionQuantitationLimitUrl","DetectionQuantitationLimitTypeName","DetectionQuantitationLimitMeasure/MeasureValue","DetectionQuantitationLimitMeasure/MeasureUnitCode",null,null,"LabSamplePreparationUrl","LastUpdated","ProviderName"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303448","Sample-Routine","Water","Surface Water","2012-11-19","10:25:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05485605",null,"L-3250012 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 101000  per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY2/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-OK","USGS Oklahoma Water Science Center","nwisok.01.01300353","Sample-Routine","Water","Surface Water","2012-11-28","11:37:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-07159735",null,"L-3340023 LC8285 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107222450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY3/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301736","Sample-Routine","Water","Surface Water","2012-12-05","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05373005",null,"L-3420030 X = LC8252 deleted per request from WSC Bode, PG, 12/7/12   Received December 06, 2012  Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235052","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300359","Sample-Routine","Water","Surface Water","2012-11-28","11:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01391100",null,"L-3340075 LC8252 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01306829","Sample-Routine","Water","Surface Water","2012-12-11","12:40:00","MST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394847104570700",null,"L-3470006 Updated time from 1230 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107243373","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303140","Sample-Routine","Water","Surface Water","2012-12-04","12:10:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-08057410",null,"L-3400056 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301741","Sample-Routine","Water","Surface Water","2012-12-04","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05340041",null,"L-3400039 Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235727","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01303146","Sample-Routine","Water","Surface Water","2012-11-19","13:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01421640",null,"L-3250019 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 133000 per Romanok.  KB 05/13/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107213401","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300361","Sample-Routine","Water","Surface Water","2012-12-10","12:10:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01409480",null,"L-3460046 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302227","Sample-Routine","Water","Groundwater","2013-09-12","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325858082480101",null,"L-2590039 X = PHARM is not a GCV, it's a PHARM   Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  FUS btl type, smpl sent to WHOI without ASR, ASR recvd 10/29/13, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305560","Sample-Routine","Water","Groundwater","2013-07-10","09:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-350206118082401",null,"L-1920075 X = DOC is not a GCC please correct your labels..  S2437 split to 20131920165, paa, 2/19/14",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94953318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301075","Sample-Routine","Water","Groundwater","2013-09-05","14:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345927078170301",null,"L-2490157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96380393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306346","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364300119400001",null,"L-2420367 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96373953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400096","Quality Control Sample-Field Replicate","Water","Groundwater","2013-12-10","11:00:00","CST",{"$nulls":13},"USGS - Minnesota Water Science Center","MN040-450655093244701",null,"L-3450050 Added agency code per Langer.  KB 02/13/14  Samples were received chilled at the WHOI lab.  Added agency code per Langer.  KB 8/13/14",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-97038996","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300295","Sample-Routine","Water","Groundwater","2013-09-12","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405817117425401",null,"L-2560044 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96537369","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300200","Sample-Routine","Water","Groundwater","2013-08-13","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333036081442108",null,"L-2270106 Received August 14, 2013  LC1792 corrected to Scgedule 1792, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1100..  time added to ASR per radon, paa, 8/15/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95650577","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300791","Sample-Routine","Water","Groundwater","2013-08-21","14:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382825075081601",null,"A-2350143 3 drops HCl in VOC's",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104233375","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300982","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",173,"feet",208,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-421600085350001",null,"L-2420481 Received August 31, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Updated agency code from 0 to USGS per Beeler.  KB 01/21/14","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96406756","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302622","Sample-Routine","Water","Groundwater","2013-08-28","11:20:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-412307091031601",null,"L-2410170 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96416767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01304485","Sample-Routine","Water","Groundwater","2013-08-27","12:00:00","MDT",{"$nulls":4},4.95,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-402104104404501",null,"A-2420473 3 drops HCl each for schedules 4436 and 4437","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96352943","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301151","Sample-Routine","Water","Groundwater","2013-09-10","16:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345941078105001",null,"L-2550057 1 bottle leaked, 1/4 sample missing, per TAL   ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96444849","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300810","Sample-Routine","Water","Groundwater","2013-08-26","13:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382403075233201",null,"L-2400035 Received August 27, 2013",null,"Not applicable","Routine sample",null,null,4044,"USGS parameter code 82398","Submersible jet pump",null,"Submersible positive-pressure pump","NWIS-96270095","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300818","Sample-Routine","Water","Groundwater","2013-08-28","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390505075353901",null,"A-2410207 2 drops HCl in VOCs",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104234663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306550","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420003",null,"L-2630079 Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.  X = Time on sample 1001. Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible positive-pressure pump","NWIS-96557211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306408","Sample-Routine","Water","Groundwater","2013-09-11","09:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364600119460002",null,"L-2590041 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96466782","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302189","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-314733085071401",null,"L-2690200 Radon LC1369 removed from this ASR by Login, customer should do the same, paa, 10/24/13  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96617213","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305583","Sample-Routine","Water","Groundwater","2013-07-18","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363645119420901",null,"L-2060065 X = 2 empty GCVs - logged from problem cooler,relabeled remaining GCVs,paa,7/25/13    Received July 19,2013..  S2437 split to 20132060192, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94984590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303635","Sample-Routine","Water","Groundwater","2013-08-21","12:50:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-440354088560701",null,"L-2380159 Received August 23,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113295181","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302557","Sample-Routine","Water","Groundwater","2013-08-19","12:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-420158093562001",null,"L-2380248 logged from problem cooler, GCVs and PHARM missing date and time, paa added, WSC notified, paa, 8/26/13  Samples were received chilled at the WHOI lab.  logged from problem cooler, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95679036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400463","Quality Control Sample-Field Replicate","Water","Groundwater","2013-12-12","10:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370500120250001",null,"L-3470071 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106778047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305546","Sample-Routine","Water","Groundwater","2013-07-08","12:50:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-381100121200501",null,"L-1900067 S2437 split to 20131900098, paa, 2/19/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94889338","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300162","Sample-Routine","Water","Groundwater","2013-05-06","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392726119460101",null,"L-1280032 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131280085, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94501761","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306400","Sample-Routine","Water","Groundwater","2013-09-10","10:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364316119360801",null,"L-2540014 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-112097888","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300815","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382906075215101",null,"A-2400162 2 drops HCl in VOCs  Sample for Sch 1792",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96270551","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01300822","Sample-Routine","Water","Groundwater","2013-08-21","12:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420410111490401",null,"L-2350034 Received August 22, 2013    per Sue changed state and county codes  pwg  2013/09/16   Updated UC from UT per Masbruch.  KB 09/19/13..  Sta ID changed from 420410111490501 to 420410111490401 per Thiros, paa, 12/31/13  Samples were received chilled at the WHOI lab.   per Sue changed state an",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104187844","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301280","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303501087174801",null,"L-2610137 Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96718520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WV","USGS West Virginia Water Science Center","nwiswv.01.01300175","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393418078132201",null,"L-2330053 User Code VA changed to WV per A. Melberg, paa, 9/10/13  Begin date is missing in mandatory field, time = 1100, JNV  Samples were received chilled at the WHOI lab...  date added to ASR per NWQL ASRs, paa, 9/3/13..  User Code VA changed to WV per A. Melberg, paa, 9/10/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96337686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302223","Sample-Routine","Water","Groundwater","2013-09-16","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323842083393201",null,"L-2600160 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300051","Sample-Routine","Water","Groundwater","2013-06-25","14:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-343817079353709",null,"L-1770065 S2437 split to 20131770134, paa, 2/18/14  Corrected invalid LC1792 to Sch1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94764758","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300739","Sample-Routine","Water","Groundwater","2013-08-14","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390217076181401",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95458314","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300873","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","EDT",{"$nulls":6},"Below land-surface datum",270,"feet",280,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380147076351201",null,"L-2620149 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96501873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306542","Sample-Routine","Water","Groundwater","2013-09-18","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363700119590001",null,"L-2630166 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300196","Sample-Routine","Water","Groundwater","2013-08-28","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351113089513401",null,"A-2410226 2 drops HCl added to VOCs  Actual radon sample collection time: 1245 CDT (estimated + 30minutes) L-2410226 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96508627","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301210","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","CDT",{"$nulls":4},92,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-412538089215801",null,"L-2400205 Date & time added to ASR per btls, paa, 8/28/13  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96070182","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305615","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364356119374001",null,"L-2070169 PEST split to separate ASR @0931, paa 7/26/13  Received July 25, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95228768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306395","Sample-Routine","Water","Groundwater","2013-09-09","13:50:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364316119360101",null,"L-2540016 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96466310","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400292","Sample-Routine","Water","Groundwater","2013-12-03","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500119590001",null,"L-3380016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306537","Sample-Routine","Water","Groundwater","2013-09-16","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363100120050002",null,"L-2610093 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098446","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303380","Sample-Routine","Water","Groundwater","2013-07-31","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-453247088425701",null,"L-2130212 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113285583","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302857","Sample-Routine","Water","Groundwater","2013-09-03","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304603094101801",null,"L-2470133 Updated STAID from 304303094101701 as per Patty 10.23.14 MKS.  btl type is FUS, paa Samples were received chilled at the WHOI lab.  per Ging changed station id from 304303094101701   pwg  2013/09/07",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96436969","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301147","Sample-Routine","Water","Groundwater","2013-09-09","12:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345005078493601",null,"L-2550061 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300824","Sample-Routine","Water","Groundwater","2013-08-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-380022079025601",null,"L-2390043 Btl type for 2255 is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96294530","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305557","Sample-Routine","Water","Groundwater","2013-07-11","08:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-353833117424001",null,"L-1960027 Received Jul 12, 2013..  S2437 split to 20131960099, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94952873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302931","Sample-Routine","Water","Groundwater","2013-07-09","10:00:00","MDT",{"$nulls":4},21,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-410251102024201",null,"L-1930027 Received Jul 11, 2013..  S2437 split to 20131930237, paa, 2/20/14",null,"Not applicable","Routine sample",null,null,4080,"USGS parameter code 82398","Peristaltic pump",null,"Peristaltic pump","NWIS-94914690","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300321","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300719092294901",null,"L-2260165 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95515272","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300673","Sample-Routine","Water","Groundwater","2013-06-13","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",377,"feet",412,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312952089444201",null,"L-1650003 S2437 split to 20131650193, paa, 2/14/14  Field alk added per manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94718189","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302856","Sample-Routine","Water","Groundwater","2013-09-04","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305947093395001",null,"L-2480032 FA condition changed to improper preservation, JNV   Lab acidification lab code 3105 added, JNV   FA preserved by C.harris on 9/11/13 @ 10:38, JNV  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301259","Sample-Routine","Water","Groundwater","2013-09-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361224076514501",null,"L-2690094 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96580242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303070","Sample-Routine","Water","Groundwater","2013-09-12","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-281433097191300",null,"L-2560186 X = 1 4437 recvd broken GCV   Updated SID from 281418097193901 per Ging.  KB 8/5/14  ASRs recvd late & entered 1/21/14, paa   Updated SID from 281418097193901 per Ging.  KB 8/20/14  Updated SID from 281418097193901 per Ging.  KB 8/5/14  btl type is FUS, paa Samples were received chilled at",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96922915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300056","Sample-Routine","Water","Groundwater","2013-07-02","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352613088381501",null,"A-1860092 2 drops of HCl in VOCs  Actual radon collection time: 1325 L-1860092 S2437 split to 20131860105, paa, 2/19/14  Samples were received chilled at the WHOI lab.","McNairy Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95009041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306409","Sample-Routine","Water","Groundwater","2013-09-11","13:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364400119450002",null,"L-2590043 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-112098073","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01303480","Sample-Routine","Water","Groundwater","2013-07-30","11:30:00","MDT",{"$nulls":4},39,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-401544103443101",null,"A-2140130 5 drops HCl each for schedules 4436 and 4437","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95388806","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303412","Sample-Routine","Water","Groundwater","2013-08-14","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-433136089235301",null,"L-2270168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113289140","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300049","Sample-Routine","Water","Groundwater","2013-06-24","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-340823079514509",null,"L-1760159 S2437 split to 20131760221, paa, 2/18/14  Corrected invalid LC1792 to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94764296","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306341","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-29","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363700119550001",null,"L-2420364 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112097698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01301828","Sample-Routine","Water","Groundwater","2013-09-23","12:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392322094214601",null,"A-2670053 VOC's HAVE 3 DROPS HCL EACH VIAL  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres.  w/2mL NITRIC ACID <pH2  RADON SAMPL   (Mailed in Fed-Ex Box) alone   Sampled @ 1440",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96605644","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300438","Sample-Routine","Water","Groundwater","2013-08-28","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301312093094101",null,"L-2410172 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96361016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300729","Sample-Routine","Water","Groundwater","2013-07-23","08:30:00","CDT",{"$nulls":6},"Below land-surface datum",358,"feet",400,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-340658088425101",null,"L-2060078 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95323181","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300690","Sample-Routine","Water","Groundwater","2013-07-17","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-391832075560801",null,"L-2040031 Received July 19, 2013..  S2437 split to 20132040231, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94987707","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300106","Sample-Routine","Water","Groundwater","2013-08-07","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-331822081020809",null,"L-2210179 Received August 08, 2013  Corrected invalid LC1792 to schedule 1792, WSC emailed, paa, 8/26/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95412663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01400050","Sample-Routine","Water","Groundwater","2013-10-29","10:40:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-402504093364301",null,"A-3030141 VOC'S HAVE 3 DROPS HCL EACH VIAL  GW-RADCHEM--(6)- 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Box Alone)   Sampled @ 1240",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96766746","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300482","Sample-Routine","Water","Groundwater","2013-09-12","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303404091325402",null,"L-2560167 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96471666","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302623","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-293938095561301",null,"L-2190145 Sta ID corrected from 561400 to 561301 per Ging,paa,9/10/13  Missing fields mandatory for WHOI,paa Samples were received chilled at the WHOI lab.  X = Time not on RADON  Sta ID corrected from 561400 to 561301 per Ging,paa,9/10/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95466090","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300115","Sample-Routine","Water","Groundwater","2013-07-17","12:00:00","EDT",{"$nulls":4},490,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-360626083170401",null,"A-2000117 3 drops of HCL added to VOCs  Actual Radon Time: 1309 L-2000117 Received July 18, 2013..  S2437 split to 20132000305, paa, 3/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95443580","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300280","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394147119580801",null,"L-2380143 Received August 23,2013..  invalid med code GW corrected to WG, paa, 8/31/13  Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96429683","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300326","Sample-Routine","Water","Groundwater","2013-08-14","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-295446091403901",null,"L-2270150 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95516191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300789","Sample-Routine","Water","Groundwater","2013-08-19","11:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383056075500201",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95663386","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300911","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","CDT",{"$nulls":6},"Below land-surface datum",283,"feet",323,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334100088193001",null,"L-2420356 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96364177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306278","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","PDT",{"$nulls":4},96,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380204",null,"L-2340193 Received August 21, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96074450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400070","Sample-Routine","Water","Groundwater","2013-10-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335943085032801",null,"L-2970176 LC1369 deleted from this ASR, paa  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96755304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300276","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375224117145401",null,"L-2410074 Received August 28, 2013..  invalid med code GW corrected to WG, paa, 9/5/13  Received August 28, 2013  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96429232","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300944","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","EDT",{"$nulls":4},38,"feet",null,35,"feet",55,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-395259083561501",null,"L-2350169 Received August 22, 2013  Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96540973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300111","Sample-Routine","Water","Groundwater","2013-08-05","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311928085494201",null,"L-2180068 Samples were received chilled at the WHOI lab.","Tallahatta Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96823327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300224","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-15","09:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322025111033101",null,"L-1970157 S2437 split to 20131970172, paa, 3/13/14  Samples leaked a little cpm <20 7/16/13, TAL  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94987231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300979","Sample-Routine","Water","Groundwater","2013-08-27","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",53,"feet",83,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435200084280001",null,"L-2410118 Btl type is FUS, paa Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96406114","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300200","Sample-Routine","Water","Groundwater","2013-08-22","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350108089242401",null,"A-2380070 2 drops HCl added to VOCs L-2380070 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96510398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302194","Sample-Routine","Water","Groundwater","2013-09-23","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312235084095301",null,"L-2670020 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96631329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302183","Sample-Routine","Water","Groundwater","2013-08-29","18:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-314356084375901",null,"L-2420348 Received August 30, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96603610","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300058","Sample-Routine","Water","Groundwater","2013-06-25","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361802088194201",null,"A-1770042 H2S odor present     2 drops HCl in VOCs  H2S odor present     Actual sample collection time 1145 L-1770042 H2S odor present cmt added per Jim, paa, 6/26/13..  S2437 split to 20131770131, paa, 2/18/14  H2S odor present cmt added per Jim, paa, 6/26/13  Samples were received chilled at the W","McNairy Formation","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95009647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300140","Sample-Routine","Water","Groundwater","2013-08-20","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350253089323901",null,"L-2330060 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96423743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303373","Sample-Routine","Water","Groundwater","2013-07-23","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-461703088043901",null,"L-2060132 Received July 24, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113282579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305665","Sample-Routine","Water","Groundwater","2013-07-23","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364259119385402",null,"L-2060023 Received July 24, 2013..  GWMSA added to ASR for WSC,paa,8/2/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95324858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302626","Sample-Routine","Water","Groundwater","2013-08-21","10:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-431045095413901",null,"L-2350103 X = Sta id on sample 431118095401.  Updated station ID from 431118095413401 as per Shannon Stubbs, KMS11/07/2013  Samples were received chilled at the WHOI lab.  Updated station ID from 431118095413401 as per Shannon Stubbs, KMS11/07/2013  Updated SID from 431118095415401 per Stubbs.  KB 0",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96422865","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301069","Sample-Routine","Water","Groundwater","2013-08-29","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344323076451301",null,"L-2420331 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96378056","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300243","Sample-Routine","Water","Groundwater","2013-07-24","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305500091065201",null,"L-2070072 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95082355","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300150","Sample-Routine","Water","Groundwater","2013-07-31","12:00:00","EDT",{"$nulls":4},0,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351019084365501",null,"A-2130165 2 drops of HCL added to VOCs  Actual Radon time = 1325 L-2130165 Updated SID from 351002084372001 per Kingsbury.  KB 09/30/13  Samples were received chilled at the WHOI lab.  Updated SID from 351002084372001 per Kingsbury.  KB 09/30/13",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-96435297","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01400144","Sample-Routine","Water","Groundwater","2013-12-03","10:45:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384457091271701",null,"L-3390014 per Paul GWMSA added, pwg  Invalid NAWQA proposal corrected, paa Samples were received chilled at the WHOI lab.  X=1 GCV vial recvd empty    per Paul GWMSA added, pwg",null,"Not applicable","Not applicable",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-96973874","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300693","Sample-Routine","Water","Groundwater","2013-07-17","13:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-392359075370301",null,"L-2040030 Received July 19, 2013..  S2437 split to 20132040230, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94988152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301074","Sample-Routine","Water","Groundwater","2013-09-05","11:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345730078301702",null,"L-2490348 4436 vial 2 GCV not recvd, ASR time changed to match btls per Fitzgerald, paa, 9/6/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-11","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300118","Sample-Routine","Water","Groundwater","2013-08-21","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321505086104601",null,"L-2350054 Received August 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96911961","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302677","Sample-Routine","Water","Groundwater","2013-08-21","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303000095002001",null,"L-2350179 Received August 22, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = Date on sample 8/12/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95677221","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300163","Sample-Routine","Water","Groundwater","2013-09-11","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333924086352901",null,"L-2550119 verified HFL recvd, not indicated as shipped, paa, 9/24/13..  sta id changed to 333924086352701 per Gill, paa, 10/30/13  ASRs recvd late & entered 1/21/14, paa     corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab..  sta id changed to 333924086352","Fort Payne Chert/formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97173275","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300969","Sample-Routine","Water","Groundwater","2013-08-07","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345051078012103",null,"L-2240084 Received August 9, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95454344","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400243","Sample-Routine","Water","Groundwater","2013-11-20","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370200120280001",null,"L-3290106 X=a PEST is a PEST, not a GCV    Received November 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775206","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300788","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382439079344801",null,"L-2340310 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95670220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300708","Sample-Routine","Water","Groundwater","2013-07-24","12:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383231075383101",null,"L-2070134 Received July 25, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95056279","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300922","Sample-Routine","Water","Groundwater","2013-09-25","14:00:00","EDT",{"$nulls":4},259,"feet",null,575.5,"feet",796,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372148076461001",null,"L-2700161 Received September 26, 2013  ASR future smpl date of 20130928 corrected to match Radon as 20130925, paa, 9/30/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96616244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300108","Sample-Routine","Water","Groundwater","2013-08-06","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335103080230801",null,"L-2190076 Samples were received chilled at the WHOI lab.  Sch 1792, not LC, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95413151","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301856","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","EDT",{"$nulls":4},45,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310913084195301",null,"L-2190136 Updated time from 110000  per Buell.  KB 10/24/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95654715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302114","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-310552084435601",null,"L-2210148 Received August 08, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96549892","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305542","Sample-Routine","Water","Groundwater","2013-07-10","13:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365516120033401",null,"L-1930108 Received July 11, 2013..  S2437 split to 20131930245, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94887660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300090","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314647085333501",null,"L-2320155 Updated SID from 314658085331201 per Gill.  KB 4/11/14  One bottle did not list date & time per TALWA, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.     corrected station id per Gill   pwg  04/18/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96811163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303649","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452733089435101",null,"L-2550111 X = Time on DOC is 1201, the rest of the bottles have the correct time  ASRs recvd late & entered 1/21/14, paa  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113298638","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300832","Sample-Routine","Water","Groundwater","2013-08-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-374426079211101",null,"L-2400078 Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107025926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302915","Sample-Routine","Water","Groundwater","2013-09-09","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-260204097443701",null,"L-2530042 Updated STAID from 260212097444301 as per Patty 10.23.14 MKS.  ASRs recvd late & entered 1/21/14, paa. Updated STAID from 260212097444301 as per Patty 10.23.14 MKS.  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301260","Sample-Routine","Water","Groundwater","2013-09-24","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362244077015501",null,"L-2690096 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96580695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301389","Sample-Routine","Water","Groundwater","2013-09-16","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-440435091404901",null,"A-2600163 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6) - 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Exact Time: 1149  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2600163 Samples were received chilled at the W",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96491554","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300294","Sample-Routine","Water","Groundwater","2013-08-14","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312658109360401",null,"L-2270082 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95513823","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302651","Sample-Routine","Water","Groundwater","2013-09-16","10:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-412938092380601",null,"L-2610026 Received September 17, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96490482","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400291","Sample-Routine","Water","Groundwater","2013-12-03","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365100120060001",null,"L-3380013 X=a PEST is a PEST not a GCV. FA is not labeled with date/time and station id  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776092","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302966","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271843098401101",null,"L-2620041 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96495760","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300151","Sample-Routine","Water","Groundwater","2013-07-18","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310630085355601",null,"L-2000277 X = No station id on samples..  S2437 split to 20132000313, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = No station id on sample",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97057695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305888","Sample-Routine","Water","Groundwater","2013-08-14","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372505",null,"L-2270202 FA btl condition changed to improper preservation, JNV   Lab acidification lab code 3105 added, JNV    FA preserved by C.Harris on 8/19/13 @ 1005, JNV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95540441","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303021","Sample-Routine","Water","Groundwater","2013-09-24","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292923095091601",null,"L-2690194 Received September 25, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96555387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300612","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","CDT",{"$nulls":4},23,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444747096272001",null,"L-2700146 X = Improper sample container for DOC btl w/teal cap    Received September 26, 2013..   invalid NAWQA proposal corrected to CL13NAWSD to complete log in of custom requests and bill properly,paa,10/22/13  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab.  P",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96726466","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301328","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-400021077303101",null,"L-2540079 ASRs recvd late & entered 1/21/14, paa  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  FED EX LATE DELIVERY",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96409324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303382","Sample-Routine","Water","Groundwater","2013-08-01","14:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-454258088411601",null,"L-2140187 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113286444","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303433","Sample-Routine","Water","Groundwater","2013-08-05","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-433215088010001",null,"L-2190094 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113292256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400071","Sample-Routine","Water","Groundwater","2013-11-04","14:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380139077212901",null,"L-3090023 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96837255","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303647","Sample-Routine","Water","Groundwater","2013-09-09","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-442100089030001",null,"L-2530033 X = RU, FU, FCC & DOC have no time on sample  ASRs recvd late & entered 1/21/14, paa  Sta id on btl different from ASR per WHOI, sta id on btl 44210008930001, paa, 10/25/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113298176","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-11","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301226","Sample-Routine","Water","Groundwater","2013-09-17","15:45:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353143076575701",null,"L-2630119 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110390359","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301225","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351119076404801",null,"L-2630111 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110389902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300220","Sample-Routine","Water","Groundwater","2013-06-27","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-321321110450101",null,"L-1790118 S2437 split to 20131790271, paa, 2/18/14  Bottles have sample time @ 11:30, per TAL, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1130",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94867231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301403","Sample-Routine","Water","Groundwater","2013-09-24","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-454805096280901",null,"A-2690071 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM-- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH 2  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1311  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-2690071 Received September 25, 2013  Sample",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96552179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300687","Sample-Routine","Water","Groundwater","2013-07-16","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384152075290401",null,"L-1990092 Received July 17, 2013..  S2437 split to 20131990205, paa, 3/14/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104083149","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300198","Sample-Routine","Water","Groundwater","2013-08-15","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-334021079501308",null,"L-2310081 S1792 not LC1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95650087","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300050","Sample-Routine","Water","Groundwater","2013-06-26","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-342455080045509",null,"L-1780152 S2437 split to 20131780189, paa, 2/18/14  Invalid LC1792 corrected to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94849214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305612","Sample-Routine","Water","Groundwater","2013-07-25","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364457119553501",null,"L-2100109 S2437 PEST split to separate ASR @1331, paa, 7/29/13    Received July 26, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95227473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01400375","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-13","10:00:00","CST",{"$nulls":4},268,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-293516098325501",null,"L-3180136 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible helical rotor pump","NWIS-96944992","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301271","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-402058076124101",null,"L-2390146 Samples were received chilled at the WHOI lab.  sta id corrected from 40305 to 40205 per Low, paa, 1/3/14",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96051022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301230","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343855078315701",null,"L-2680058 Received September 24, 2013  Samples were received chilled at the WHOI lab.  X = recvd without ASR Eric faxed",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96504664","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302221","Sample-Routine","Water","Groundwater","2013-09-17","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323336084050601",null,"L-2610069 X = A PHARM is not a GCV  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96701634","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01301819","Sample-Routine","Water","Groundwater","2013-09-30","10:20:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-402332091342901",null,"L-2970126 Login delayed due to gov shutdown, ok to log recvd 10/24 from Paul B., paa, 10/24/13   Received October 01, 2013  File recvd late from TAL, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96604163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300082","Sample-Routine","Water","Groundwater","2013-07-15","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-313139085402101",null,"L-1990008 X = Samples do not have station id    Received July 16, 2013..  S2437 split to 20131990194, paa, 3/13/14  Samples were received chilled at the WHOI lab.  X = Station id not on label","Providence Sand","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96795508","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301395","Sample-Routine","Water","Groundwater","2013-09-18","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-435217095063401",null,"A-2620087 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6) - 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1155  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2620087 Samples were received chilled at the",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96492675","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300133","Sample-Routine","Water","Groundwater","2013-08-12","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-322405087342601",null,"L-2250122 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96912544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300324","Sample-Routine","Water","Groundwater","2013-08-27","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-353232114200501",null,"L-2400155 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96279525","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300919","Sample-Routine","Water","Groundwater","2013-09-26","10:00:00","EDT",{"$nulls":4},100,"feet",null,190,"feet",208,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372823076433601",null,"L-2950071 Login delayed due to gov shutdown, ok log per B.Lindsey, paa, 10/22/13    Received September 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible helical rotor pump","NWIS-96615768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300945","Sample-Routine","Water","Groundwater","2013-09-30","12:00:00","EDT",{"$nulls":4},315,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-381531076583001",null,"L-2950073 Login delayed due to gov shutdown,ok log per B. Lindsey,paa,10/22/13   Received October 1,2013  File recvd late from TAL, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96781492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302202","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321838084435101",null,"L-2660027 Received September 20, 2013  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96633103","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01400374","Sample-Routine","Water","Groundwater","2013-11-14","09:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292331098294501",null,"L-3220033 Received November 15, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-96944555","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300070","Sample-Routine","Water","Groundwater","2013-07-30","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322643087020001",null,"L-2130003 Updated SID from 322644087020201 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14","Coker Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96776124","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300431","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324858109510701",null,"L-2320058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97321453","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303450","Sample-Routine","Water","Surface Water","2013-05-20","12:15:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05451210",null,"L-1410060 Evn. ASR & smpls changed to 1215 per K.Romanok, paa, 5/21/13..  LC8252 deleted per Rose, paa, 5/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY155/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300913","Sample-Routine","Water","Groundwater","2013-08-28","14:30:00","CDT",{"$nulls":6},"Below land-surface datum",2210,"feet",2280,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332240089033401",null,"L-2410237 Samples were received chilled at the WHOI lab.  X = Time on samples 1430..  time added to ASR per radon, paa, 9/5/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96364801","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01303486","Sample-Routine","Water","Groundwater","2013-07-31","11:40:00","MDT",{"$nulls":4},5.8,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-402213104015501",null,"A-2140132 6 drops HCl each for schedules 4436 and 4437.","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95387948","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301149","Sample-Routine","Water","Groundwater","2013-09-10","10:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341758077480802",null,"L-2550063 X = No time on RU  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443932","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306349","Sample-Routine","Water","Groundwater","2013-08-27","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364400119450001",null,"L-2470093 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96371045","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303418","Sample-Routine","Water","Groundwater","2013-08-07","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444302089144401",null,"L-2210439 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113290029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301223","Sample-Routine","Water","Groundwater","2013-09-17","08:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350717077002001",null,"L-2630113 X = Date on samples 9-17-13  Updated date from 2013/09/13 per Pointer.  KB 12/16/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110388985","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306358","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363500120030001",null,"L-2410019 Received August 28, 2013  Samples were received chilled at the WHOI lab.  smdugan added, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96371910","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300174","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","CDT",{"$nulls":4},98,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350543089473901",null,"A-2270007 3 drops HCl added to VOCs L-2270007 Received August 14, 2013  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96464256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301348","Sample-Routine","Water","Groundwater","2013-09-12","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-463618094183101",null,"A-2560042 VOCs HAVE 5 DROPS HCL EACH VIAL   Pleas lab filter schedule 2434  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH 2   LC=1364, LC=2164, shipped in 2nd cooler  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Actual time = 1335  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96448793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303374","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-460308088130601",null,"L-2110172 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300582","Sample-Routine","Water","Groundwater","2013-06-05","11:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385009075444401",null,"L-1580144 Received June 6, 2013,  STA ID corrected to 385009075444401 per Bringman GB 9/3/13..  S2437 split to 20131580152, paa, 2/14/14  STA ID corrected to 385009075444401 per Bringman GB 9/3/13",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94559591","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303377","Sample-Routine","Water","Groundwater","2013-07-30","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-451854087545501",null,"L-2130206 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113284297","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306281","Sample-Routine","Water","Groundwater","2013-08-20","09:00:00","PDT",{"$nulls":4},148,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380203",null,"L-2340191 Received August 21, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96159326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400078","Sample-Routine","Water","Groundwater","2013-10-24","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345255085174201",null,"L-3010111 Received October 25, 2013..  LC1369 removed from this ASR, paa, 11/4/13  Btl type FUS, not GCC, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96763067","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300404","Sample-Routine","Water","Groundwater","2013-08-21","12:00:00","MST",{"$nulls":4},75,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325104109421001",null,"L-2350253 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96935655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400457","Sample-Routine","Water","Groundwater","2013-12-09","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700119470002",null,"L-3450047 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776976","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302563","Sample-Routine","Water","Groundwater","2013-08-13","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-421016092020201",null,"L-2260157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95679968","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305541","Sample-Routine","Water","Groundwater","2013-07-11","10:10:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365418120035101",null,"L-1970165 S2437 split to 20131970173, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94887240","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301224","Sample-Routine","Water","Groundwater","2013-09-17","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350513076501501",null,"L-2630121 One btl recvd without label per Testam, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110389445","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301269","Sample-Routine","Water","Groundwater","2013-09-24","16:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351731076514101",null,"L-2700088 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110393177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301685","Sample-Routine","Water","Groundwater","2013-08-19","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414400112050001",null,"L-2330051 ASR missing med code and smpl type, WG/9 added per PEST ASR, paa, 8/29/13  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-95681871","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01302838","Sample-Routine","Water","Groundwater","2013-09-18","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-393922096114901",null,"L-2630162 X = 1 GCV has date 9/?/2013  Btl type for Sch2255 i FUS, paa Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97186914","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301207","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":4},17,"feet",null,20,"feet",28,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-411432088234001",null,"L-2390164 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95912157","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301861","Sample-Routine","Water","Groundwater","2013-08-08","12:30:00","EDT",{"$nulls":4},22,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-311015084511901",null,"A-2210433 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-95668982","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300052","Sample-Routine","Water","Groundwater","2013-07-10","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354601084084201",null,"A-1930090 3 drops HCL added to VOC's  Actual Sample Time = 13:03 L-1930090 Received July 11, 2013   X = Please do not use pencil on ASR..  S2437 split to 20131930241, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94977484","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300286","Sample-Routine","Water","Groundwater","2013-09-04","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393351116000101",null,"L-2490177 Corrected med code to WG, paa   Recvd 9/6/13  Recvd 9/6/13  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96467946","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400242","Sample-Routine","Water","Groundwater","2013-11-19","10:20:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370800120270001",null,"L-3240015 X=PEST is PEST not GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300433","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310305092101202",null,"L-2400177 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96360558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300064","Sample-Routine","Water","Groundwater","2013-07-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-332036079244009",null,"L-2000084 Received July 18, 2013..  S2437 split to 20132000304, paa, 3/14/14  Corrected LC1792 to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94954827","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400459","Sample-Routine","Water","Groundwater","2013-12-10","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370200119590001",null,"L-3450049 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300169","Sample-Routine","Water","Groundwater","2013-08-14","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335323088074301",null,"L-2270136 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97177368","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WV","USGS West Virginia Water Science Center","nwiswv.01.01300172","Sample-Routine","Water","Groundwater","2013-08-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392158077525301",null,"L-2320020 X = Samples have date 8-19-13   Begin date is missing in mandatory field, time = 1100, JNV..  date added to ASR per btls, paa, 8/26/13..  User Code VA changed to WV per A. Melberg, paa, 9/10/13  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  User Code VA changed to WV",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96337224","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306534","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420001",null,"L-2610074 Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96538536","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301628","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401012111354801",null,"L-2270198 Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95475574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300238","Sample-Routine","Water","Groundwater","2013-07-23","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302602091002505",null,"L-2060069 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95081886","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303022","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-291949095024801",null,"L-2690191 Received September 25, 2013  Updated SID from 292037095010501 per Ging.  KB 8/5/14  FUS btl type, paa Samples were received chilled at the WHOI lab.  Received September 25, 2013   Updated SID from 292037095010501 per Ging.  KB 8/5/14  Updated SID from 292037095010501 per Ging.  KB 8/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921974","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305563","Sample-Routine","Water","Groundwater","2013-07-09","08:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-333700114340001",null,"L-1910081 S2437 split to 20131910107, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96048698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302169","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320051084061401",null,"A-2270163 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96562950","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301263","Sample-Routine","Water","Groundwater","2013-09-25","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355840076571001",null,"L-2730028 Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96582061","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300942","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",177,"feet",197,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-403857082191101",null,"L-2270191 Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96559910","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303632","Sample-Routine","Water","Groundwater","2013-08-21","17:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-442008089135201",null,"L-2380161 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113294745","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400072","Sample-Routine","Water","Groundwater","2013-10-23","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-341529085071301",null,"L-2970178 LC1369 deleted from this ASR, paa  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96754845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300115","Sample-Routine","Water","Groundwater","2013-09-11","08:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333642086065001",null,"L-2550121 X  =Time on samples 0900..  verified HFL recvd, not indicated as shipped, paa, 9/12/13   Updated SID from 333642086065101 per Gill.  KB 4/11/14  ASRs recvd late & entered 1/21/14, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.     corre",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96888911","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303415","Sample-Routine","Water","Groundwater","2013-08-08","15:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435453089184701",null,"L-2210437 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113289584","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300114","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-315522087045901",null,"L-2330058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96889501","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300316","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354709115220001",null,"L-2680157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96730762","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300326","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-353513114161701",null,"L-2410259 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96280146","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300336","Sample-Routine","Water","Groundwater","2013-09-04","09:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320138111165301",null,"L-2480050 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96400549","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300330","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345516114364901",null,"L-2420145 FED EX LATE DELIVERY  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96278913","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305216","Sample-Routine","Water","Groundwater","2013-06-10","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-372100118250001",null,"L-1620245 S2437 split to 20131620256, paa, 2/14/14  GWMSA added due to exception, paa, 6/13/13  Samples were received chilled at the WHOI lab.  D-R'd per Mullin, sample ruined at contract lab.  KB 10/29/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94737897","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305596","Sample-Routine","Water","Groundwater","2013-07-15","10:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-345006118125701",null,"L-1990052 Received July 16, 2013..  S2437 split to 20131990197, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95016292","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303376","Sample-Routine","Water","Groundwater","2013-07-25","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452121088541301",null,"L-2110168 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01400007","Sample-Routine","Water","Groundwater","2013-11-06","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375700114254801",null,"L-3110028 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96891758","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300910","Sample-Routine","Water","Groundwater","2013-09-23","14:00:00","EDT",{"$nulls":6},"Below land-surface datum",279,"feet",354,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-374550077300501",null,"L-2680054 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96614340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302212","Sample-Routine","Water","Groundwater","2013-09-17","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323316084140501",null,"L-2610067 X = PHARM is not a GCV  Btl type is FUS, ASR missing mandatory pH, paa, 10/28/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96701171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301404","Sample-Routine","Water","Groundwater","2013-09-26","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-454900094342101",null,"L-2730066 Received September 27, 2013  Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96552765","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303656","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-432700089440001",null,"L-2350223 X = Date on samples 8/21/2013   Updated date from 2013/08/22 per Manteufel.  KB 02/03/14  Samples were received chilled at the WHOI lab.  radon recvd without smpl info on cylinder or smpl, added label per ASR, WSC emailed, paa, 8/22/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113299165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301258","Sample-Routine","Water","Groundwater","2013-09-23","14:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354953076484101",null,"L-2690100 X = GCV vial recvd broken  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96579784","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301266","Sample-Routine","Water","Groundwater","2013-09-23","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352301077300701",null,"L-2700086 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110391808","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300955","Sample-Routine","Water","Groundwater","2013-07-09","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352832076470102",null,"L-1920048 RECEIVED JULY 10, 2013..  S2437 split to 20131920163, paa, 2/19/14    X = Please correct your btl labels for SCH 2437, pest & LC 9017 Pharm.  They are not GCV's   LC's not indicated as add or delete, LC's added.  CSH  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-103032770","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301790","Sample-Routine","Water","Groundwater","2013-09-11","08:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394200111490001",null,"L-2550014 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96440191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300741","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","CDT",{"$nulls":6},"Below land-surface datum",832,"feet",863,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342409088520901",null,"L-2100009 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95379365","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305616","Sample-Routine","Water","Groundwater","2013-07-22","14:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363806119345301",null,"L-2050201 Received July 23, 2013..  S2437 split to 20132050229, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95229190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301148","Sample-Routine","Water","Groundwater","2013-09-09","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343726078360201",null,"L-2550065 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443472","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301154","Sample-Routine","Water","Groundwater","2013-09-12","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352839077040701",null,"L-2560053 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110388041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300735","Sample-Routine","Water","Groundwater","2013-07-24","15:45:00","CDT",{"$nulls":6},"Below land-surface datum",1609,"feet",1689,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345216089400201",null,"L-2100003 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95378132","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306533","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-17","09:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420002",null,"L-2610076 Samples were received chilled at the WHOI lab..  Sta ID changed to 364200119420002 per Dugan, paa, 3/21/14",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96538091","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300281","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-385738119433601",null,"L-2320053 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96428784","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300161","Sample-Routine","Water","Groundwater","2013-07-16","11:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312534085203401",null,"L-1990082 X = No station id on samples    Received July 17, 2013..  S2437 split to 20131990199, paa, 3/13/14  Updated SID from 312517085201801 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.     corrected station id per Gill   pwg  04/18/14  X = You need to put station id on yo",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97172773","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300285","Sample-Routine","Water","Groundwater","2013-09-03","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392933117061701",null,"L-2470086 invalid med code GW corrected to WG, WSC notified, paa, 9/7/13  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96467494","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300676","Sample-Routine","Water","Groundwater","2013-06-25","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",315,"feet",345,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311642090113601",null,"L-1780043 Received June 26, 2013..  S2437 split to 20131780187, paa, 2/18/14  Received June 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94780770","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301071","Sample-Routine","Water","Groundwater","2013-09-03","16:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344734077254601",null,"L-2490159 Radon recvd completely unlabeled, added label per ASR, WSC notified requesting verify, paa, 9/4/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96378578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300717","Sample-Routine","Water","Groundwater","2013-07-30","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-393254075531801",null,"L-2130017 Received July 31, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95321788","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305213","Sample-Routine","Water","Groundwater","2013-06-11","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-342953117173101",null,"L-1630037 S2437 split to 20131630117, paa, 2/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94738454","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300137","Sample-Routine","Water","Groundwater","2013-09-16","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-334821086090001",null,"L-2610031 X = Improper sample container for RU in 1L glass bottle  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96918391","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300292","Sample-Routine","Water","Groundwater","2013-08-15","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-314322110030901",null,"L-2280189 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95513204","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300118","Sample-Routine","Water","Groundwater","2013-07-18","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355047084082701",null,"A-2030048 Drops of HCl added to VOCs  Actual Radon Time: 1212 L-2030048 Received July 19, 2013..  S2437 split to 20132030166, paa, 3/17/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95444192","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300170","Sample-Routine","Water","Groundwater","2013-08-20","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350403089445201",null,"L-2330062 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96463385","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300894","Sample-Routine","Water","Groundwater","2013-09-16","11:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393241077434201",null,"L-2600149 Updated UC from PA per Dieter.  KB 11/18/13  2 caps broken, sample for alpha beta empty, per testam, paa  Updated UC from PA per Dieter.  KB 11/18/13  Samples were received chilled at the WHOI lab.  Updated UC from PA per Dieter.  KB 11/18/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Other","NWIS-96479376","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300141","Sample-Routine","Water","Groundwater","2013-05-01","14:45:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392927119475201",null,"L-1230039 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131230103, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94382991","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300674","Sample-Routine","Water","Groundwater","2013-06-19","11:15:00","CDT",{"$nulls":6},"Below land-surface datum",210,"feet",250,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315920089541701",null,"L-1710186 S2437 split to 20131710195, paa, 2/18/14  1369 is lab code, not schedule, paa  Chg'd to S1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94772526","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301167","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","CDT",{"$nulls":6},"Below land-surface datum",18,"feet",28,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393232088221801",null,"L-2320066 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95545324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305682","Sample-Routine","Water","Groundwater","2013-07-30","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364639120065001",null,"L-2130124 S2437 deleted from this ASR, see 2nd ASR @1331 for PEST, paa, 8/10/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95371649","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300704","Sample-Routine","Water","Groundwater","2013-07-23","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-374755075371001",null,"L-2060179 Received July 24, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95055836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300425","Sample-Routine","Water","Groundwater","2013-09-05","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324937113304501",null,"L-2490270 X = Time on samples 1100  Samples were received chilled at the WHOI lab.  X = Time on sample 1100",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97320825","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300208","Sample-Routine","Water","Groundwater","2013-08-14","14:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350018089190701",null,"A-2270187 2 drops HCl added to VOCs L-2270187 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96511276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300206","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350625089554901",null,"A-2410042 2 drops HCl/VOC vial L-2410042 Received August 28, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96509517","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300145","Sample-Routine","Water","Groundwater","2013-04-29","11:15:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391126119423201",null,"L-1210155 Lab codes not indicated as add or delete, LC's added, JNV..  one GCV converted to PEST and added, prog code corrected to GWMSA WSC notified, paa, 5/2/13..  S2437 split to 20131210174, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94425121","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300204","Sample-Routine","Water","Groundwater","2013-09-11","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351231089392301",null,"A-2550041 2  drops HCl/VOC vial L-2550041 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96510832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303023","Sample-Routine","Water","Groundwater","2013-09-23","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300932094005301",null,"L-2680148 Received September 24, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96555820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306553","Sample-Routine","Water","Groundwater","2013-09-24","11:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364100119440001",null,"L-2680178 Smpl type changed from 1 to 9 per Evans, paa, 9/25/13     DOC condition changed to improper preservation, JNV  Samples were received chilled at the WHOI lab.  WSC emailed regarding smpl type 1, paa   Changed smpl type to 9 per Dugan, paa, 10/31/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96576242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305617","Sample-Routine","Water","Groundwater","2013-07-23","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363928119401701",null,"L-2070165 X = Station ID diff. on btls's 363928119401701  PEST split to separate ASR @ 1001, paa 7/26/13  Received July 25, 2013,  STAID changed to 363928119401701 per Bennett GB 9/3/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95232156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300785","Sample-Routine","Water","Groundwater","2013-08-15","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385634078261501",null,"L-2280112 Btl type is FUS, paa   Begin date is missing in mandatory field, time = 1100, JNV Samples were received chilled at the WHOI lab.  date added to ASR per NWQL ASR, paa, 9/7/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107025473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302965","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271505098073401",null,"L-2660071 Received September 20, 2013  Updated SID per Ging. 8/5/14  FUS btl type,paa Samples were received chilled at the WHOI lab.  Sta ID changed to 271505098073401 per Ging, paa, 9/25/14  Updated SID per Ging. 8/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921542","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306284","Sample-Routine","Water","Groundwater","2013-08-19","14:40:00","PDT",{"$nulls":4},105,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380202",null,"L-2380206 ASR sta id corrected to match btls & per Dugan and fields corrected too, paa, 8/26/13  Updated SID from 364258119380201 per Dugan.  KB 09/10/13  Lid was off of one bottle (alpha/beta) and entire volume was lost   Station id on bottle is: 364258119380202   ASR sta id corrected per Dugan",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96074884","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300221","Sample-Routine","Water","Groundwater","2013-07-10","11:15:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333051112082001",null,"L-1930036 Received Jul 11, 2013..  S2437 split to 20131930238, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94924871","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303378","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-30","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-454107088011001",null,"L-2130208 S2437 deleted from this ASR, see second @1331, paa, 8/10/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113284726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300348","Sample-Routine","Water","Groundwater","2013-08-19","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313610091504501",null,"L-2320151 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95555138","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300277","Sample-Routine","Water","Groundwater","2013-07-30","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-344152111592301",null,"L-2130032 Received July 31, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95389988","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302554","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-430449096061301",null,"L-2380244 logged from problem cooler, paa  Samples were received chilled at the WHOI lab.  logged from problem cooler, smpl information added to GCVs by paa, 8/26/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95678562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300088","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314038085365401",null,"L-2390168 X = Time on sample 1200",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96801601","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01301526","Sample-Routine","Water","Surface Water","2013-05-13","11:40:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-324305097101900",null,"L-1350041 Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY257/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300666","Sample-Routine","Water","Groundwater","2013-07-08","14:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-373330075494601",null,"L-1920036 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131920161, paa, 2/19/14",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94892623","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300167","Sample-Routine","Water","Groundwater","2013-07-24","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-321100086344501",null,"L-2070098 Received July 25, 2013..  PEST and S2437 split to second ASR @1130, Lab ID 20132070161, paa, 7/26/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97176757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300696","Sample-Routine","Water","Groundwater","2013-07-18","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385715075253001",null,"L-2030146 Received July 19, 2013..  S2437 split to 20132030167, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-94988597","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300331","Sample-Routine","Water","Groundwater","2013-08-15","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-312038092192601",null,"L-2280129 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95515726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306344","Sample-Routine","Water","Groundwater","2013-08-28","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364100119450001",null,"L-2420373 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96373509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300053","Sample-Routine","Water","Groundwater","2013-07-15","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353857084511801",null,"A-1990033 3 drops HCl added to VOCs  Actual Radon Sample Time: 14:13 L-1990033 Received July 16, 2013..  S2437 split to 20131990196, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94978083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301372","Sample-Routine","Water","Surface Water","2013-03-12","15:20:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02281200",null,"L-0730004 Updated time from 1500 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107230079","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-03-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY264/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302859","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-280951096593801",null,"L-2410129 FUS btl type, paa Samples were received chilled at the WHOI lab.  Lid was completely off one sample, but lost small amount of sample (aprox 150-175mLs) per Test Am, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368442","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PR","USGS Puerto Rico Water Science Center","nwispr.01.01301107","Sample-Routine","Water","Surface Water","2013-03-19","10:40:00","AST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-50055410",null,"L-0790103 Updated time from 103000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107219605","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-03","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY266/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302621","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292944095550101",null,"L-2210241 Received August 08, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = Time of sample label 1006",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95465216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300086","Sample-Routine","Water","Groundwater","2013-07-08","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323528086205801",null,"L-1900068 S2437 split to 20131900099, paa, 2/19/14  Samples were received chilled at the WHOI lab.  X = Please put information on tube so that we do not have to open, PG","Coker Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96800988","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300297","Sample-Routine","Water","Groundwater","2013-09-10","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-404325116065801",null,"L-2540077 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300100","Sample-Routine","Water","Groundwater","2013-08-08","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355752082564201",null,"A-2210431 3 drops of HCL added to VOCs  Actual Radon time =  1334 L-2210431 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95426613","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300736","Sample-Routine","Water","Groundwater","2013-07-24","12:45:00","CDT",{"$nulls":6},"Below land-surface datum",492,"feet",552,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343706089111601",null,"L-2100006 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95378734","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302619","Sample-Routine","Water","Surface Water","2013-04-16","10:10:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02335870",null,"L-1080111 Received April 17, 2013  Updated time from 100000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107221194","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY272/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300599","Sample-Routine","Water","Groundwater","2013-06-12","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390126075575401",null,"L-1640024 S2437 split to 20131640198, paa, 2/14/14",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94621681","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305207","Sample-Routine","Water","Groundwater","2013-06-13","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-335700116300001",null,"L-1690057 X = 9017 PHARM & 2434 HFL are not GCV's    Received June 14, 2013..  S2437 split to 20131690165, paa, 2/18/14  Samples were received chilled at the WHOI lab.  Updated SID from 33570011630001 per Dugan.  KB 07/11/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95906708","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300153","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-16","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354041084243601",null,"A-1990083 3 drops of HCL added to VOCs  Radon actual time = 1244 L-1990083 X = Please do not use pencil on ASR   Received July 17, 2013  Samples were received chilled at the WHOI lab.  corrected eASR sta id for Creekside per G. Johnson,paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96436487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302165","Sample-Routine","Water","Groundwater","2013-08-13","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312346084520401",null,"L-2270074 Received August 14, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96562393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400295","Sample-Routine","Water","Groundwater","2013-12-05","09:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370000120120001",null,"L-3400054 station id corrected per Sue D.  pwg 1/02/14  Samples were received chilled at the WHOI lab.   corrected station id per Sue D.  pg  5/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776798","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300202","Sample-Routine","Water","Groundwater","2013-09-12","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350327089421401",null,"A-2560154 2 drops HCl/VOC vial L-2560154 only 5 GCV vials recvd per Murtaugh, paa  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96509069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300668","Sample-Routine","Water","Groundwater","2013-07-10","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-380403075292901",null,"L-1960088 Received July 12, 2013..  S2437 split to 20131960102, paa, 2/20/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94893474","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300148","Sample-Routine","Water","Groundwater","2013-08-14","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350234089394504",null,"A-2270189 2 drops HCl added to VOCs L-2270189 Updated SID from 350235089394701 per Kingsbury.  KB 09/30/13  Samples were received chilled at the WHOI lab.  Updated SID from 350235089394701 per Kingsbury.  KB 09/30/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96425510","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302862","Sample-Routine","Water","Groundwater","2013-08-21","16:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301420095093201",null,"L-2350194 Received August 22, 2013    Per Ging changed station id from 301419095093301   pwg  2013/09/07  FUS btl type, paa Samples were received chilled at the WHOI lab.  Received August 22, 2013. Updated STAID from 301419095093301 as per Patty 10.23.14 MKS.  Updated STAID from 301419095093301 as p",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96369313","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301624","Sample-Routine","Water","Groundwater","2013-08-15","12:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401148112433002",null,"L-2310079 Samples were received chilled at the WHOI lab.","Valley Fill","Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible piston pump","NWIS-95475102","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300193","Sample-Routine","Water","Groundwater","2013-05-08","11:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391111119481901",null,"L-1340062 Received May 11, 2013..  S2437 split to 20131340161, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4060,"USGS parameter code 82398","Gas reciprocating pump",null,"Gas reciprocating pump","NWIS-94586331","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300270","Sample-Routine","Water","Groundwater","2013-08-06","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304612089512401",null,"L-2200021 Received August 7, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95430262","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300314","Sample-Routine","Water","Groundwater","2013-09-19","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405517114204101",null,"L-2630098 DOC condition changed to improper preservation, JNV  sta id correction per K. Thomas,paa,11/4/13  Samples were received chilled at the WHOI lab.  sta id correction per K. Thomas,paa,11/4/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96602216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01400009","Sample-Routine","Water","Groundwater","2013-11-07","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361200115580001",null,"L-3120076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96939011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300198","Sample-Routine","Water","Groundwater","2013-09-10","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351528089350801",null,"A-2540036 2 drops HCl added to VOCs L-2540036 ASRs recvd late & entered 1/21/14, paa..  Sta ID changed to 351528089350801 per Kingsbury, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96509954","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303381","Sample-Routine","Water","Groundwater","2013-08-01","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-462416088191901",null,"L-2140189 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113286014","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305585","Sample-Routine","Water","Groundwater","2013-07-17","10:50:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363107119372201",null,"L-2000067 Received July 18, 2013..  S2437 split to 20132000302, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985015","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301228","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-18","12:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354552077382301",null,"L-2630064 Samples were received chilled at the WHOI lab.  corrected station id per WSC  pwg  1/30/814  smpl type 9 corrected to 7 per Erik, paa, 10/31/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96503748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300792","Sample-Routine","Water","Groundwater","2013-08-21","09:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384322075394401",null,"L-2350145 Received August 22, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104233803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301152","Sample-Routine","Water","Groundwater","2013-09-11","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343908078432003",null,"L-2550059 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96445309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302855","Sample-Routine","Water","Groundwater","2013-09-05","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310935093352701",null,"L-2490137 FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96367572","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300428","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-314050091260501",null,"L-2380072 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96360106","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300985","Sample-Routine","Water","Groundwater","2013-08-29","09:00:00","EDT",{"$nulls":6},"Below land-surface datum",92,"feet",112,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-423200084490001",null,"L-2420479 Received August 31, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96407397","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301231","Sample-Routine","Water","Groundwater","2013-09-19","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342728077335701",null,"L-2680056 Received September 24, 2013  Samples were received chilled at the WHOI lab.  Updated SID from 342650077351501 per Pointer.  KB 01/10/14  X = Recvd without ASR Erik faxed corrected btl label per Brian, PG",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96505120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302620","Sample-Routine","Water","Groundwater","2013-08-08","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-290028095594700",null,"L-2210360 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = 1 FA recvd  X = Time on sample 1032",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95464775","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300298","Sample-Routine","Water","Groundwater","2013-09-11","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405030115500001",null,"L-2550083 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573942","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300300","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312423110574901",null,"L-2190150 Updated SID from 312443110573001 per Beisner.  KB 01/02/14  Dropped and cracked lids on 2 bottles during receipt. Lost small amount of volume. Transferred to new containers per TALWA      Updated SID from 312443110573001 per Beisner.  KB 01/02/14  Samples were received chilled at the WHOI",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95530757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305259","Sample-Routine","Water","Groundwater","2013-06-25","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-333130114394001",null,"L-1770062 DOC changed to improper preservation, paa..  GWMSA added, WSC to verify, paa, 6/29/13..  S2437 split to 20131770132, paa, 2/18/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125523816","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300149","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342640088065901",null,"L-1980064 X = No station id on samples..  S2437 split to 20131980174, paa, 3/13/14  Samples were received chilled at the WHOI lab.  X=Station ID not on label",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97057093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300723","Sample-Routine","Water","Groundwater","2013-07-11","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",1989,"feet",2074,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333618089074301",null,"L-1960028 Received Jul 12, 2013..  S2437 split to 20131960100, paa, 2/20/14  Received Jul 12,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95237689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305540","Sample-Routine","Water","Groundwater","2013-07-11","12:50:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365220120052601",null,"L-1970151 S2437 split to 20131970169, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94886821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301068","Sample-Routine","Water","Groundwater","2013-08-28","11:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344244077135801",null,"L-2420333 X = Only 2 GCVs for 4436 recvd  Few samples had loose lids and leaked. COCs were not in plastic bag and got soaked per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96377603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01400231","Sample-Routine","Water","Groundwater","2013-12-11","10:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302329087040001",null,"L-3460042 FUS btl typpe for S2255, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97164340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301073","Sample-Routine","Water","Groundwater","2013-09-04","14:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351804077520101",null,"L-2490155 ASR missing mandatory pH & alk, paa Samples were received chilled at the WHOI lab.  Per Shanon F.  corrected station id.  pwg  1/13/2014",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300721","Sample-Routine","Water","Groundwater","2013-07-09","10:45:00","CDT",{"$nulls":6},"Below land-surface datum",1480,"feet",1546,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325846088340801",null,"L-1910088 S2437 split to 20131910109, paa, 2/19/14  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95236492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300988","Sample-Routine","Water","Groundwater","2013-09-03","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",93,"feet",113,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-424900083150001",null,"L-2480071 Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96408037","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300976","Sample-Routine","Water","Groundwater","2013-08-26","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",150,"feet",185.8,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435000084510001",null,"L-2410124 Lab Codes not indicated as add or delete,lab codes added,AAN  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Samples received 8/29/13 @ 1015 am, 45 minutes left to run 2hr alpha beta per Test Am, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96405475","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305897","Sample-Routine","Water","Groundwater","2013-08-13","13:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372501",null,"L-2260083 Corrected to GWMSA, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95531694","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300746","Sample-Routine","Water","Groundwater","2013-07-23","12:30:00","CDT",{"$nulls":6},"Below land-surface datum",1303,"feet",1383,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341359089062201",null,"L-2060081 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95380599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400289","Sample-Routine","Water","Groundwater","2013-12-02","09:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365400120070001",null,"L-3380015 X=a PEST is a PEST, not a GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775737","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300135","Sample-Routine","Water","Groundwater","2013-08-15","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-332357087524301",null,"L-2280114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96913142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300219","Sample-Routine","Water","Groundwater","2013-07-01","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-325329112405301",null,"L-1840085 Received July 2,2013..  S2437 split to 20131840130, paa, 2/19/14  Released Gross alpha beta per Mullin.  KB 6/17/15  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94866626","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300916","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","EDT",{"$nulls":4},210,"feet",null,247,"feet",272,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372148076461002",null,"L-2700159 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96615293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300142","Sample-Routine","Water","Groundwater","2013-08-27","18:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350514089553700",null,"A-2410044 3 drops of HCl added to VOCs L-2410044 Received August 28, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96424178","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400018","Sample-Routine","Water","Groundwater","2013-10-28","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",477,"feet",538,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375541076514301",null,"L-3030063 Received October 29, 2013  Samples were received chilled at the WHOI lab.  sta id corrected to 4301 per A. Melberg, paa, 1/21/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96781964","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NE","USGS Nebraska Water Science Center","nwisne.01.01300271","Sample-Routine","Water","Surface Water","2013-06-10","10:10:00","CDT",{"$nulls":14},"USGS-06770195",null,"L-1640193 Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY318/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302645","Sample-Routine","Water","Groundwater","2013-09-18","10:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-415613094591201",null,"L-2620166 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96489562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301072","Sample-Routine","Water","Groundwater","2013-09-04","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344002077013201",null,"L-2490161 Samples were received chilled at the WHOI lab.  X = Date on sample 9/4/13..  ASR date corrected to match Radon, paa, 9/7/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300223","Sample-Routine","Water","Groundwater","2013-07-18","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-330135111231701",null,"L-2000244 S2437 split to 20132000307, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = Time on sample 1110",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-97152093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305593","Sample-Routine","Water","Groundwater","2013-07-16","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-344400117200001",null,"L-1990012 Received July 17, 2013..  S2437 split to 20131990195, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95016762","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301270","Sample-Routine","Water","Groundwater","2013-09-26","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354245077311701",null,"L-2730032 Received September 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110393632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306539","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364300119420001",null,"L-2610095 Missing alk, WSC emailed, 10/31/13, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400240","Sample-Routine","Water","Groundwater","2013-11-18","10:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370500120190001",null,"L-3240012 X=PEST is not GCV it is a PEST  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106774675","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305543","Sample-Routine","Water","Groundwater","2013-07-10","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365700120063401",null,"L-1930105 Received July 11, 2013    Btl type for S2437 is PEST,  paa..  S2437 split to 20131930242, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94888080","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300155","Sample-Routine","Water","Groundwater","2013-08-07","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-315820087202001",null,"L-2210136 Updated SID from 315915087202301 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97167396","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300879","Sample-Routine","Water","Groundwater","2013-09-19","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",618,"feet",659,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-373759076345501",null,"L-2660019 Received September 20, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96502818","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302200","Sample-Routine","Water","Groundwater","2013-09-18","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320859085003701",null,"L-2620156 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96632654","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400076","Sample-Routine","Water","Groundwater","2013-10-29","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344855084461101",null,"L-3030172 LC1369 removed from this ASR, paa, 11/4/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96762615","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400074","Sample-Routine","Water","Groundwater","2013-11-05","10:00:00","EST",{"$nulls":4},307,"feet",null,850,"feet",985,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365751076363001",null,"L-3100037 Date on btls 11/5/13..  corrected ASR date to match per A. Melberg, paa, 1/21/14  WSC emailed to verify field alk, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab...  field alk updated to 419.5 per Teunis, WHOI updated, paa, 11/13/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96837725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400027","Sample-Routine","Water","Groundwater","2013-10-31","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",215,"feet",316,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372105077113601",null,"L-3080057 Received November 1, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96783378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300066","Sample-Routine","Water","Groundwater","2013-07-10","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320848080454301",null,"L-1920128 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131920167, paa, 2/19/14  1792 is schedule, not lab code, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94955751","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","improper preservationsample was dilutedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300613","Sample-Routine","Water","Groundwater","2013-09-24","10:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-445330097071801",null,"L-2700147 X= Improper sample container for DOC btl w/teal cap    Received September 26, 2013..   invalid NAWQA proposal corrected to CL13NAWSD to complete log in of custom requests and bill properly,paa,10/22/13  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab. Sam",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96727024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301171","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-21","11:00:00","CDT",{"$nulls":4},60,"feet",null,77,"feet",102,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-383932090012601",null,"L-2350123 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95555768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300275","Sample-Routine","Water","Groundwater","2013-07-29","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-342557112041303",null,"L-2120035 PEST & Sch2437 split to second ASR, paa, 7/31/13   Time not on PHARM, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95389378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302198","Sample-Routine","Water","Groundwater","2013-09-24","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320348084132701",null,"L-2680108 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96632220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300265","Sample-Routine","Water","Groundwater","2013-07-31","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301407092104201",null,"L-2130178 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Grab sample","NWIS-95420211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300068","Sample-Routine","Water","Groundwater","2013-07-16","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333850079014308",null,"L-1990137 Received July 17, 2013     GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131990208, paa, 3/14/14  LC1792 corrected to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94990374","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300296","Sample-Routine","Water","Groundwater","2013-07-16","09:45:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315010111000701",null,"L-1990053 Received July 17, 2013..  S2437 split to 20131990198, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-95529513","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302914","Sample-Routine","Water","Groundwater","2013-09-10","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271315097473201",null,"L-2540057 1 cap broken, 3/4 sample missing per TAL   ASRs recvd late & entered 1/21/14, paa  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96454122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306555","Sample-Routine","Water","Groundwater","2013-09-25","13:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364306119364401",null,"L-2700140 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96575802","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303639","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-460000088235501",null,"L-2400181 Bottles have station id of 460000088265501, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113295868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400074","Sample-Routine","Water","Groundwater","2013-10-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-343914085165901",null,"L-3010107 Received October 25, 2013..  LC1369 removed from this ASR, paa, 11/4/13  Btl type is FUS, not GCC, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96762152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300147","Sample-Routine","Water","Groundwater","2013-05-07","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-393023119513701",null,"L-1300100 Received May 09, 2013..  S2437 split to 20131300206, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94424715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300060","Sample-Routine","Water","Groundwater","2013-06-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-360010088252901",null,"A-1780184 2 drops HCl in VOCs  H2S in sample  Actual sample collection time 0945 L-1780184 S2437 split to 20131780191, paa, 2/18/14  Samples were received chilled at the WHOI lab.","McNairy Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95010258","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305656","Sample-Routine","Water","Groundwater","2013-07-25","11:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364338119354602",null,"L-2110122 Received July 26, 2013..  NAWQA program code GWMSA added to ASR,paa,8/9/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95325321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300144","Sample-Routine","Water","Groundwater","2013-08-28","14:30:00","CDT",{"$nulls":4},76,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351111089512501",null,"A-2410228 2 drops HCl added to VOC  Actual radon collection time: 1631 CDT L-2410228 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96424621","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302858","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-290209096302701",null,"L-2420230 FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96369796","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300402","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-13","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-314204110224201",null,"L-2260076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96937465","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301688","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414233112174501",null,"L-2340074 X = Time on samples 1300, 1 GCV broken in cooler during shipping    Received August 21, 2013  Samples were received chilled at the WHOI lab.  X = Time on sample 1300",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible positive-pressure pump","NWIS-95682330","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300190","Sample-Routine","Water","Groundwater","2013-08-07","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363025082070401",null,"A-2250034 3 drops of HCL added to VOCs, H2S positive sniff test  Actual Radon time = 1311  H2S detected L-2250034 Received August 9, 2013  Samples were received chilled at the WHOI lab.  Updated date from 2013/08/06 per Kingsbury.  KB 3/7/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96472864","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300084","Sample-Routine","Water","Groundwater","2013-07-17","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311805085462401",null,"L-2000053 Received July 18, 2013..  S2437 split to 20132000301, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = You need station id on labels","Providence Sand","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96802205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400290","Sample-Routine","Water","Groundwater","2013-12-02","12:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365200119560001",null,"L-3380014 X=a PEST is a PEST, not a GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306287","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","PDT",{"$nulls":4},70,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380201",null,"L-2320034 One bottle has lid broken off, and all sample is missing  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96075341","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302045","Sample-Routine","Water","Surface Water","2013-07-23","09:10:00","EST",{"$nulls":14},"USGS-02350524",null,"L-2060191 Received July 24, 2013  Deleted LC 8252 per Rose.  KB 09/16/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107104896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY356/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300318","Sample-Routine","Water","Groundwater","2013-09-30","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-364912114041201",null,"L-2940041 Login delayed due to gov shutdown,ok log per Bexfield,paa,10/21/13    Received October 1,2013  File recvd late from TAL, paa  Login delayed due to gov shutdown, ok log per Bexfield, paa, 10/21/13    Received October 1, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96731658","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301282","Sample-Routine","Water","Groundwater","2013-09-18","11:00:00","CDT",{"$nulls":4},320,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305708087091201",null,"L-2620069 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96718991","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300051","Sample-Routine","Water","Groundwater","2013-07-09","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351253085105801",null,"A-1910015 Actual Sample Time 13:30 L-1910015 S2437 split to 20131910104, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94976882","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300065","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-325447080383601",null,"L-1970152 Received July 12, 2013..  S2437 split to 20131970170, paa, 3/13/14  Samples were received chilled at the WHOI lab.  Schedule 1792, not LC, paa",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94955288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305590","Sample-Routine","Water","Groundwater","2013-07-17","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-351556116404601",null,"L-1990171 S2437 split to 20131990210, paa, 3/14/14  1 bottle had no time, TAL  Only smpl identification on RADON is 0936, logged by paa from problem cooler, paa, 7/18/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95015806","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300734","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","CDT",{"$nulls":6},"Below land-surface datum",925,"feet",1025,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345021088572201",null,"L-2110047 Received July 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95377529","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KY","USGS Kentucky Water Science Center","nwisky.01.01300436","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365200088210001",null,"L-2620048 X = FCC has no time, a PHARM is not a GCV    per Angie changed station ID and name  pwg  2013/09/26..  Sta ID changed to 365200088210001 per A. Crain, paa, 2/7/14  Samples were received chilled at the WHOI lab.  Updated SID from 365147088205702 and added station name per Crain.  KB 01/07/1",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96970314","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300477","Sample-Routine","Water","Groundwater","2013-09-11","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304921092402202",null,"L-2550097 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96471207","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301405","Sample-Routine","Water","Groundwater","2013-09-10","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",48,"feet",88,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-400026091242501",null,"L-2540101 ASRs recvd late & entered 1/21/14,paa  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96432919","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300956","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-24","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350012077131101",null,"L-2110205 Corrected ST to GWMSA, paa   Received July 27, 2013..  S2437 deleted from this ASR, invalid S2612 corrected to LC2612, paa, 8/9/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95362122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305613","Sample-Routine","Water","Groundwater","2013-07-25","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364312119592901",null,"L-2100107 S2437 & PEST split to separate ASR @1001, paa, 7/29/13    Received July 26, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95227896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305891","Sample-Routine","Water","Groundwater","2013-08-14","10:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372504",null,"L-2270210 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95531246","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300722","Sample-Routine","Water","Groundwater","2013-07-10","10:50:00","CDT",{"$nulls":6},"Below land-surface datum",1135,"feet",1185,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-331358088350001",null,"L-1920073 S2437 split to 20131920164, paa, 2/19/14  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95237088","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MT","USGS Montana Water Science Center","nwismt.01.01301628","Sample-Routine","Water","Surface Water","2013-08-28","10:40:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05014300",null,"L-2410104 Deleted 8252 per Rose.  KB 11/21/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107100098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY370/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306428","Sample-Routine","Water","Groundwater","2013-09-12","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363500120000001",null,"L-2590046 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098261","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305246","Sample-Routine","Water","Groundwater","2013-06-17","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-331211116185101",null,"L-1690111 X = btl type for Sch2437 is PEST, not GCV   Updated SID from 331200116180001 per Dugan.  KB 07/12/13  Sta id on btl 331200116180001 per WHOI, paa Samples were received chilled at the WHOI lab.  Updated SID from 331200116180001 per Dugan.  KB 07/12/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94758029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302483","Sample-Routine","Water","Groundwater","2013-06-26","15:15:00","MDT",{"$nulls":4},10,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-405159102444201",null,"L-1790275 S2437 split from 20131790260, paa, 2/18/14","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94803537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302861","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-291639097093901",null,"L-2400044 Received August 27, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300112","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352745084341201",null,"A-1970120 3 drops HCl in VOCs  Actual Sample Time = 13:08 L-1970120 X = Please do not use electrical tape on DOC sample    Received July 12, 2013  Updated SID from 352741084342001 and date from 20130712 per Kingsbury.  KB 3/7/14.. S2437 split to 20131970166, paa, 3/13/14  Samples were received chill",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96472245","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301866","Sample-Routine","Water","Groundwater","2013-08-12","18:00:00","EDT",{"$nulls":4},38,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-314858084194901",null,"A-2250046 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-95669666","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400293","Sample-Routine","Water","Groundwater","2013-12-04","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500120110001",null,"L-3400053 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776452","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300913","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","EDT",{"$nulls":4},164,"feet",null,200,"feet",220,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372454076512801",null,"L-2680168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96614817","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300248","Sample-Routine","Water","Groundwater","2013-07-24","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303001090274201",null,"L-2070070 Received July 25, 2013  Samples were received chilled at the WHOI lab.  X = Time sensitive time 1545",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95082821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301221","Sample-Routine","Water","Groundwater","2013-09-16","12:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345637076383501",null,"L-2630115 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96503293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300967","Sample-Routine","Water","Groundwater","2013-08-07","16:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343308077484501",null,"L-2240086 Received August 9, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95453906","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302936","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-11","10:30:00","CDT",{"$nulls":4},11,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-410959100582401",null,"L-1930218 S2437 split to 20131930249, paa, 2/20/14",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94915432","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300669","Sample-Routine","Water","Groundwater","2013-07-10","14:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-380027075410802",null,"L-1960087 Received July 12, 2013..  S2437 split to 20131960101, paa, 2/20/14  Even though samples lids were taped, some still leaked. JB 7/12/13 < 20cpm, TAL",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94893899","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302913","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-275725097562701",null,"L-2550106 ASRs recvd late & entered 1/21/14, paa  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96453689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305582","Sample-Routine","Water","Groundwater","2013-07-18","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363726119465201",null,"L-2030161 Received July 19, 2013..  S2437 split to 20132030169, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94984167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306275","Sample-Routine","Water","Groundwater","2013-08-21","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363337120070001",null,"L-2340269 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96158873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305545","Sample-Routine","Water","Groundwater","2013-07-09","10:10:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-381031121123901",null,"L-1930106 Received July 11, 2013..  S2437 split to 20131930243, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94888921","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400294","Sample-Routine","Water","Groundwater","2013-12-04","12:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365900120040001",null,"L-3400052 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776625","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300941","Sample-Routine","Water","Groundwater","2013-08-13","15:00:00","EDT",{"$nulls":6},"Below land-surface datum",52,"feet",67,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-394208082252201",null,"L-2270196 Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96559417","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305586","Sample-Routine","Water","Groundwater","2013-07-16","14:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363317119490401",null,"L-1990088 Btl type for S2437 is PEST not GVPEST, paa    Received July 17, 2013..  S2437 split to 20131990201, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985439","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301265","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-401002078254801",null,"L-2340287 GWMSA added, btl types corrected, paa, 8/22/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Other","NWIS-95667915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300839","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-371444080012701",null,"L-2400080 Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96295016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301261","Sample-Routine","Water","Groundwater","2013-09-24","15:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361252077074501",null,"L-2690102 4 bottles show sample date as 9/24/13. 9-23 will be used, per TestAm, paa..  ASR date corrected from 20130923 to 20130924 per Pointer, paa, 2/10/14  Samples were received chilled at the WHOI lab.  X= Date on sample 9/24/13..  ASR date corrected from 20130923 to 20130924 per Pointer, paa, 2",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96581152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306352","Sample-Routine","Water","Groundwater","2013-08-27","09:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364600119460001",null,"L-2410021 Received August 28,2013  2 of the bottles did not have station id #, date or time, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96374398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305210","Sample-Routine","Water","Groundwater","2013-06-12","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-341643116243101",null,"L-1640078 S2437 split to 20131640200, paa, 2/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94737449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300328","Sample-Routine","Water","Groundwater","2013-08-26","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-335825112435301",null,"L-2390103 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96280759","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300218","Sample-Routine","Water","Groundwater","2013-07-02","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332149113124601",null,"L-1860005 Received July 03, 2013..  S2437 split to 20131860104, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-94866036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","sample was dilutedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400021","Sample-Routine","Water","Groundwater","2013-10-29","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365649077233801",null,"L-3030199 Samples were received chilled at the WHOI lab..  WSC emailed for sample time, WHOI did not send btl label information, paa, 11/12/13..  time of 1200 added per Teunis, paa, 11/13/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96782434","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301262","Sample-Routine","Water","Groundwater","2013-09-25","10:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353749076333501",null,"L-2730030 Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96581607","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302676","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300413094402101",null,"L-2380135 Received August 23, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95676793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301264","Sample-Routine","Water","Groundwater","2013-09-26","10:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353605077483901",null,"L-2730034 Received September 27, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96582515","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306541","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-18","08:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-363700119550002",null,"L-2630170 Mising alk, WSC emailed, paa, 10/31/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96539013","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301267","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395625077585901",null,"L-2350258 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95668381","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400081","Sample-Routine","Water","Groundwater","2013-11-07","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-364151076571701",null,"L-3160061 Received November 08, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96838196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301390","Sample-Routine","Water","Groundwater","2013-09-17","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-433617092494301",null,"A-2610085 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6)- 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Exact time: 1315  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2610085 Samples were received chilled at the WH",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96492016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300611","Sample-Routine","Water","Groundwater","2013-09-26","10:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-434704096440701",null,"L-2950077 Logged from problem cooler per Joyce,delay due to gov shutdown,paa,10/22/13  Logged from problem cooler per Joyce, delay due to gov shutdown, paa, 10/22/13  Proposal added, paa  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96725909","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301268","Sample-Routine","Water","Groundwater","2013-09-24","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350420077084901",null,"L-2700188 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110392721","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306896","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-25","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351600116030002",null,"L-2700164 Received September 26, 2013   Updated SID from 351600116030001 per Vasquez.  KB 12/18/13  Samples were received chilled at the WHOI lab.   Updated SID from 351600116030001 per Vasquez.  KB 12/18/13  Updated SID from 351600116030001 per Vasquez.  KB 12/18/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-98339431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400024","Quality Control Sample-Field Replicate","Water","Groundwater","2013-10-30","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",264,"feet",420,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-370156077063801",null,"L-3040104 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96782906","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303430","Sample-Routine","Water","Groundwater","2013-08-12","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-431953088113701",null,"L-2250078 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113291811","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300819","Sample-Routine","Water","Groundwater","2013-08-28","13:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-391233075433102",null,"A-2410209 3 drops HCl in each VOC",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104235098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300121","Sample-Routine","Water","Groundwater","2013-07-30","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352554084193001",null,"A-2130055 4 drops of HCL added to VOCs  Actual Radon time = 1426 L-2130055 Received July 31, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95444799","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301483","Sample-Routine","Water","Groundwater","2013-09-30","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-445132093392101",null,"A-2940037 VOCs HAVE 5 DROPS HCL EACH VIAL (please lab filter schedule 2434)  GW-RADCHEM -- (6) - 1 LITER BOTLLES pres w/2mL NITRIC ACID <pH2  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-2940037 Login delayed due to gov shutdown, ok log per Terrio, paa, 10/21/13   Per btl labels, lab filter a",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96578141","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306272","Sample-Routine","Water","Groundwater","2013-08-22","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363900119500001",null,"L-2350235 X = Time on Sample 1030",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112097516","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301259","Sample-Routine","Water","Groundwater","2013-08-15","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-403325077242001",null,"L-2280187 GWMSA added to ASR, paa  Sta id on btl 403325077342001 per WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95517179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300716","Sample-Routine","Water","Groundwater","2013-07-29","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-381754075083601",null,"L-2120071 Received July 30, 2013",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95321354","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300670","Sample-Routine","Water","Groundwater","2013-07-11","10:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-381245075404001",null,"L-1970136 Received July 12, 2013..  S2437 split to 20131970167, paa, 3/13/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94894327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301300","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-404510077093801",null,"L-2400098 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96162973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300279","Sample-Routine","Water","Groundwater","2013-07-31","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334657113365501",null,"L-2130098 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95390601","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400078","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-06","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365147076343001",null,"L-3110102 STA ID changed per Alyssa M 11/26/13 GB  Samples were received chilled at the WHOI lab. STA ID changed per Alyssa M 11/26/13 GB",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96943034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301150","Sample-Routine","Water","Groundwater","2013-09-10","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342300077425401",null,"L-2550067 X = Date on bottles is 9-9-13  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96444391","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301340","Sample-Routine","Water","Groundwater","2013-09-11","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395804076084801",null,"L-2550048 ASRs recvd late & entered 1/21/14, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96431820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302648","Sample-Routine","Water","Groundwater","2013-09-17","10:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-414101094303802",null,"L-2610129 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96490010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300907","Sample-Routine","Water","Groundwater","2013-08-29","14:00:00","CDT",{"$nulls":6},"Below land-surface datum",1302,"feet",1368,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332056088420901",null,"L-2420353 Received August 30, 2013  Bottles are labeled 3/29/13 1400, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96362936","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303427","Sample-Routine","Water","Groundwater","2013-08-06","13:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-443810088311601",null,"L-2190092 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113291366","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301787","Sample-Routine","Water","Groundwater","2013-09-09","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385752112225301",null,"L-2530044 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96439288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301265","Sample-Routine","Water","Groundwater","2013-09-23","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351806077434501",null,"L-2700084 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110391352","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300317","Sample-Routine","Water","Groundwater","2013-09-23","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361023115114401",null,"L-2670013 ASR time 0900 (corrected from 9000), paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96731214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303371","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-440157089180501",null,"L-2060129 Received July 24, 2013..  PEST not recvd for this ASR, S2437 deleted, see 206-130 for pest, paa, 8/2/13  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113281717","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300821","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382843078363101",null,"L-2350198 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96294072","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300028","Sample-Routine","Water","Groundwater","2013-06-12","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302120087374201",null,"L-1650045 Received June 13, 2013..  S2437 split to 20131650195, paa, 2/14/14  Sample exceeds 72hrs per TAL, paa  Samples were received chilled at the WHOI lab.  X = Need to put label on outside of tube",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-94670165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300917","Sample-Routine","Water","Groundwater","2013-08-15","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345740089141601",null,"L-2310001 Received August 16, 2013  Updated UC from TN per Kingsbury.  KB 09/11/13  Updated UC from TN per Kingsbury.  KB 09/11/13  WHOI recvd smpl without ASR originally, ASR recvd 11/8, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96423304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300727","Sample-Routine","Water","Groundwater","2013-07-22","15:45:00","CDT",{"$nulls":6},"Below land-surface datum",545,"feet",625,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342111089124401",null,"L-2040214 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95312179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400461","Sample-Routine","Water","Groundwater","2013-12-11","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370100120060001",null,"L-3470072 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301153","Sample-Routine","Water","Groundwater","2013-09-11","15:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352200077230601",null,"L-2560051 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1315",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96445767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300141","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332833086203001",null,"L-2540048 X = Date on samples 9/7/2013   Updated SID from 332849086203501 per Gill.  KB 4/11/14  Sample date on bottle says 9/17/13, per TAL    ASRs recvd late & entered 1/21/14, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.    corrected station",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96927678","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300298","Sample-Routine","Water","Groundwater","2013-07-23","09:15:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-330420112034301",null,"L-2060173 Received July 24,2013..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  Samples were received chilled at the WHOI lab.  medium code corrected from WS to WG per Beisner, paa, 8/26/13  medium code corrected from WS to WG per Beisner, paa, 8/26/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95530139","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300866","Sample-Routine","Water","Groundwater","2013-09-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-370328080263101",null,"L-2600138 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96481995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300725","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-383756078455601",null,"L-2320018 Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95514802","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305671","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119385601",null,"L-2050179 Received July 23, 2013..  GWMSA added, WSC to verify, paa, 8/2/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab...  sta id changed to 85601 per Dugan, paa, 10/30/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95327078","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300397","Sample-Routine","Water","Groundwater","2013-07-17","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332916110510201",null,"L-1990162 Updated SID from 332927110511701 per Beisner.  KB 12/13/13..  S2437 split to 20131990209, paa, 3/14/14  Samples were received chilled at the WHOI lab.  Updated SID from 332927110511701 per Beisner.  KB 12/13/13  Updated SID from 332927110511701 per Beisner.  KB 12/13/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96936255","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300067","Sample-Routine","Water","Groundwater","2013-07-09","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-324829079533000",null,"L-1910021 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131910105, paa, 2/19/14  Corrected to schedule 1792, not lab code, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94956213","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400245","Sample-Routine","Water","Groundwater","2013-11-21","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365900120140001",null,"L-3290104 X=a PEST is a PEST, not a GCV     Received November 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-106775562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301174","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","CDT",{"$nulls":4},80,"feet",null,42,"feet",82,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375756088081201",null,"L-2380075 Received August 23, 2013  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95671290","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305662","Sample-Routine","Water","Groundwater","2013-07-24","10:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364259119385404",null,"L-2070171 GWMSA added to ASR, paa, 7/26/13   Received July 25, 2013  GWMSA added to ASR,paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95326202","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303379","Sample-Routine","Water","Groundwater","2013-07-31","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-450755088125301",null,"L-2130210 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113285154","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303375","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-451805088363101",null,"L-2110170 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283440","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300092","Sample-Routine","Water","Groundwater","2013-08-28","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315244085100401",null,"L-2410140 Updated SID from 315241085100501 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14","Tuscaloosa Group","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96811766","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300159","Sample-Routine","Water","Groundwater","2013-09-04","05:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324159087362001",null,"L-2480016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97173868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300275","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302832090064101",null,"L-2210134 WHOI ASR missing alkalinity, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95430725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302577","Sample-Routine","Water","Groundwater","2013-08-27","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-423846095141801",null,"L-2400168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96069579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301229","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354838076541201",null,"L-2630062 X = Time on samples 1000  Updated time from 100100 per Giorgino.  KB 8/5/15  Samples were received chilled at the WHOI lab.  X = Time on sample 1001",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96504205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300277","Sample-Routine","Water","Groundwater","2013-08-26","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-381704117031401",null,"L-2400093 Received August 27, 2013..  invalid med code GW corrected to WG, paa, 9/5/13  Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96427889","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300296","Sample-Routine","Water","Groundwater","2013-09-16","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-401115118301501",null,"L-2600153 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300242","Sample-Routine","Water","Groundwater","2013-07-09","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-334638112314501",null,"L-1910086 Updated SID from 334639112314801per Partin.  KB 08/07/13..  S2437 split to 20131910108, paa, 2/19/14  Samples were received chilled at the WHOI lab.  Updated SID from 334639112314801per Partin.  KB 08/07/13  Updated SID from 334639112314801per Partin.  KB 08/07/13  X = Time not on sample",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95232791","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300400","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322549111191601",null,"L-2110058 Received July 26, 2013..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  Samples were received chilled at the WHOI lab..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  medium code corrected from WS to WG per Beisner, paa, 8/26/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96936858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302225","Sample-Routine","Water","Groundwater","2013-09-16","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324816083290901",null,"L-2600158 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01300594","Sample-Routine","Water","Surface Water","2013-06-18","12:10:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-13210360",null,"L-1710091 ID user code per Romanok, paa, 6/20/13  Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107112487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY458/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301844","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313415084475201",null,"L-2270076 Received August 14, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95553116","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300790","Sample-Routine","Water","Groundwater","2013-08-20","09:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384630075524801",null,"A-2330078 1 drop HCl in VOC",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95663815","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300793","Sample-Routine","Water","Groundwater","2013-08-19","14:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383100076061103",null,"L-2320038 S1792 unclear, paa, ok'd to TALWA",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95664244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300733","Sample-Routine","Water","Groundwater","2013-07-25","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",597,"feet",637,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345002088374401",null,"L-2110051 Received July 26, 2013  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95376926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300217","Sample-Routine","Water","Groundwater","2013-06-26","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321846110592801",null,"L-1790022 Received June 27, 2013..  S2437 split to 20131790270, paa, 2/18/14  GWMSA added per NWQL ASRs, paa  GWMSA added, WSC to verify, paa, 7/3/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-94846967","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301213","Sample-Routine","Water","Groundwater","2013-08-28","11:00:00","CDT",{"$nulls":4},134,"feet",null,135,"feet",150,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-422448088041901",null,"L-2410083 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96272163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300100","Sample-Routine","Water","Groundwater","2013-07-09","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325627087043401",null,"L-1910053 X = Station ID not on btl's..  S2437 split to 20131910106, paa, 2/19/14  Samples were received chilled at the WHOI lab.  X = Station ID not on sample  Need label on outside of tube",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96813135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301067","Sample-Routine","Water","Groundwater","2013-08-28","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343400077292201",null,"L-2420329 Few samples had loose lids and leaked. COCs were not in plastic bag - soaked!, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96377142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302622","Sample-Routine","Water","Groundwater","2013-08-14","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-294040096542401",null,"L-2270120 Sta ID corrected from 542400 to 542401 per Ging,paa,9/10/13  Missing fields mandatory for WHOI,paa Samples were received chilled at the WHOI lab.  X = Only one FA bottle received  Sta ID corrected from 542400 to 542401 per Ging,paa,9/10/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95465651","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300127","Sample-Routine","Water","Groundwater","2013-07-23","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361610083581801",null,"A-2060161 3 drops of HCL added to VOCs  Actual Radon time = 12:52 L-2060161 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104108276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300421","Sample-Routine","Water","Groundwater","2013-08-05","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-331616111401101",null,"L-2180154 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-97270953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300202","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335128081250001",null,"L-2340223 Samples were received chilled at the WHOI lab.  Sch 1792 not LC1792, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95651065","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300991","Sample-Routine","Water","Groundwater","2013-09-04","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",53,"feet",63,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-432500082320001",null,"L-2480069 Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96408673","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300054","Sample-Routine","Water","Groundwater","2013-06-27","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351004088351501",null,"A-1820069 3 drops HCI in VOC's  Actual Radon time = 1015 L-1820069 Received Jun 28, 2013.. S2437 split to 20131820140, paa, 2/19/14  Updated SID from 351008088350601 per Kingsbury.  KB 3/7/14  Samples were received chilled at the WHOI lab..  Sta ID changed to 351004088351501 per Kingsbury,paa,3/13/1","Eutaw Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95010864","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400462","Sample-Routine","Water","Groundwater","2013-12-11","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700120090001",null,"L-3470073 Samples were received chilled at the WHOI lab..  sta id corrected from 9001 to 90001 per Dugan, paa, 2/10/14  Updated SID from 365700120090011 per Dugan.  KB 2/28/14  sta id corrected from 9001 to 90001 per Dugan, paa, 2/10/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777863","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300668","Sample-Routine","Water","Groundwater","2013-05-30","11:15:00","CDT",{"$nulls":6},"Below land-surface datum",139,"feet",161,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-313400091210001",null,"L-1510001 S2437 split to 20131510155, paa, 2/14/14  Btl type for S2255 is FUS, paa Samples were received chilled at the WHOI lab.  Sample is outside 72hrs per TAL, paa..  corrected LC1792 to Schedule 1792,paa,7/6/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94695044","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302679","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302207096050600",null,"L-2320028 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95678095","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300940","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",65,"feet",90,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-394257082362603",null,"L-2270194 Samples were received chilled at the WHOI lab..  smpl date changed from 20130812 to 20130813 per Runkle, WHOI notified, paa, 10/28/13","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96558923","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300311","Sample-Routine","Water","Groundwater","2013-08-20","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392212119223001",null,"L-2340238 Received August 21, 2013  Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Received August 21, 2013   Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Samples were received chilled at the WHOI lab.  Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Updated SID",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96574934","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300794","Sample-Routine","Water","Groundwater","2013-08-20","13:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-385023076013501",null,"A-2330080 3 drops HCl in VOC",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104234231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300164","Sample-Routine","Water","Groundwater","2013-08-12","15:00:00","CDT",{"$nulls":4},60,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350643089502001",null,"A-2320150 2 drops of HCl added to VOCs L-2320150 Recvd without ASR originally, paa    Recvd 8/14/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96462089","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302678","Sample-Routine","Water","Groundwater","2013-08-20","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302145095473901",null,"L-2340207 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95677660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300882","Sample-Routine","Water","Groundwater","2013-09-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-365525080564901",null,"L-2620055 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96550326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302209","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323255084141801",null,"L-2610071 X = A PHARM is not a GCV  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96700736","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306394","Sample-Routine","Water","Groundwater","2013-09-09","10:40:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364316119360102",null,"L-2540012 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96465878","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301267","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353257077285302",null,"L-2700186 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110392264","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300809","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384606075115801",null,"L-2400038 Received August 27, 2013",null,"Stable, normal stage","Routine sample",null,null,4044,"USGS parameter code 82398","Submersible jet pump",null,"Submersible positive-pressure pump","NWIS-96269660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300671","Sample-Routine","Water","Groundwater","2013-06-12","15:00:00","CDT",{"$nulls":6},"Below land-surface datum",650,"feet",700,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302825089042001",null,"L-1640162 Field alk added per Manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792, paa  S2437 split to 20131640201, paa, 2/14/14  verified PHARM not recvd for this ASR, LC9017 deleted, paa, 6/18/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94716983","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301788","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373900113130001",null,"L-2540111 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96439732","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305584","Sample-Routine","Water","Groundwater","2013-07-17","14:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363418119384201",null,"L-2000068 Received July 18, 2013..  S2437 split to 20132000303, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94986606","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301168","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","CDT",{"$nulls":4},60,"feet",null,55,"feet",65,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-391127088273501",null,"L-2330040 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95545955","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300670","Sample-Routine","Water","Groundwater","2013-06-12","10:00:00","CDT",{"$nulls":6},"Below land-surface datum",530,"feet",570,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310929088334101",null,"L-1650043 Received June 13, 2013    Lab codes not indicated as add or delete, LC's added, JNV  Field alk added per Manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792 per TALWA, time on btls is 10:00, paa    Updated time from 093500 per Manning.  KB 10/10/",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94716379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301227","Sample-Routine","Water","Groundwater","2013-09-18","09:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355220076371501",null,"L-2680110 X = Recvd without ASR logged in from problem cooler Sharon faxed 9/25/13, PG  ASR not recvd with smpls, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110390817","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400087","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-20","11:00:00","CST",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-443306094125501",null,"L-3250095 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96957832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301347","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-465926093354201",null,"A-2550072 VOCs HAVE   DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH2 LC1505 and LC2170 were shipped in a 2nd cooler  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1432  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-1",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96448332","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305587","Sample-Routine","Water","Groundwater","2013-07-16","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363316119473001",null,"L-1990090 Received July 17, 2013..  S2437 split to 20131990203, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300146","Sample-Routine","Water","Groundwater","2013-08-21","15:30:00","CDT",{"$nulls":4},71,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351448089421700",null,"A-2350039 2 drops HCl added to VOC L-2350039 Received August 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96425064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300146","Sample-Routine","Water","Groundwater","2013-05-06","10:45:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392937119452601",null,"L-1280031 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131280084, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94424307","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303643","Sample-Routine","Water","Groundwater","2013-08-28","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-445647091215301",null,"L-2420148 Samples were received chilled at the WHOI lab.  Some samples had leaked. COC and cooler wet per Test Am, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113297244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300102","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320431085315301",null,"L-2050150 X = Station id not on sample    Received July 23, 2013..  S2437 split to 20132050227, paa, 3/17/14   Updated SID from 320431085315401 per Gill.  KB 4/11/14  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/","Eutaw Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96813737","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300178","Sample-Routine","Water","Groundwater","2013-09-10","08:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351315089310501",null,"A-2540042 2 drops HCl added to VOCs L-2540042 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96461585","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300876","Sample-Routine","Water","Groundwater","2013-09-18","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380103076315901",null,"L-2620114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96502347","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300280","Sample-Routine","Water","Groundwater","2013-08-08","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",635,"feet",670,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-312144092401801",null,"L-2210320 Received August 09, 2013  WHOI ASR missing alkalinity, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95431180","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300743","Sample-Routine","Water","Groundwater","2013-07-23","16:15:00","CDT",{"$nulls":6},"Below land-surface datum",343,"feet",423,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341519088393901",null,"L-2060085 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95379978","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305610","Sample-Routine","Water","Groundwater","2013-07-16","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362921119335901",null,"L-1990089 Received July 17, 2013,  STA ID changed from 362621119335901 to 362921119335901 per Bennett GB..  S2437 split to 20131990202, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95074449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302479","Sample-Routine","Water","Groundwater","2013-06-24","14:20:00","MDT",{"$nulls":4},9.5,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-400237104500301",null,"L-1770009 LC not indicated as add or delete, LC added, JD..  S2437 split to 20131770130, paa, 2/18/14",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94804423","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302191","Sample-Routine","Water","Groundwater","2013-09-25","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312332084555101",null,"L-2690202 ASR missing mandatory alk, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96617648","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303372","Sample-Routine","Water","Groundwater","2013-07-23","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-461739087192201",null,"L-2060131 Received July 24, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113282145","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01402392","Sample-Routine","Water","Groundwater","2014-08-21","11:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-464418119432901",null,"L-2380179 Received August 22, 2014  Received August 22,2014",null,"Not applicable","Not applicable",null,null,4047,"USGS parameter code 82398","Submersible gear pump",null,"Submersible gear pump","NWIS-99204203","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400284","Sample-Routine","Water","Surface Water","2014-04-15","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214655255",null,"A-1070012 10 min time offset",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97702315","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY648/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400378","Sample-Routine","Water","Surface Water","2014-04-16","10:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0208524090",null,"A-1070135 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97747492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY654/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401154","Sample-Routine","Water","Surface Water","2014-06-11","13:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02095181",null,"L-1690057 Received June17, 2014",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98459973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY673/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401199","Sample-Routine","Water","Surface Water","2014-06-11","16:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0212430653",null,"L-1690092 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98477301","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY692/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401205","Sample-Routine","Water","Surface Water","2014-06-11","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0212467595",null,"A-1680169 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98478357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY711/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01402223","Sample-Routine","Water","Groundwater","2014-06-10","10:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322018108392501",null,"L-1620192 S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98532731","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400735","Sample-Routine","Water","Surface Water","2014-05-13","10:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02085500",null,"L-1360081 Received May 15, 2014..  ASR date changed from 20140512 to 20140513 per Cassy P,paa,6/6/14",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97955558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",0.04,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400798","Sample-Routine","Water","Groundwater","2014-01-13","15:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380302121203201",null,"L-0150012 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-112099668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-01-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404355","Sample-Routine","Water","Groundwater","2014-08-18","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361207121075501",null,"L-2330026 Received August 20, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-105560148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01400898","Sample-Routine","Water","Groundwater","2014-07-31","13:00:00","EST",{"$nulls":6},"Below land-surface datum",null,null,170,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382556078565401",null,"L-2130077 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98823072","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-06","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01400484","Sample-Routine","Water","Groundwater","2014-05-12","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",1245,"feet",1325,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323308090180901",null,"L-1330111 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-97966196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01402806","Sample-Routine","Water","Groundwater","2014-08-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-294345094364501",null,"L-2320022 Received August 19, 2014  S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab.  X=time on pest is 1400   Received August 19, 2014",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99090184","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401189","Sample-Routine","Water","Surface Water","2014-06-10","14:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214265808",null,"L-1690115 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98465895","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY870/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01403520","Sample-Routine","Water","Groundwater","2014-08-20","10:00:00","MDT",{"$nulls":13},"USGS - Colorado Water Science Center","USGS-365802105313101",null,"L-2340267 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-104282190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402295","Sample-Routine","Water","Groundwater","2014-07-15","11:00:00","CST",{"$nulls":4},230,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-441948088094901",null,"L-1970139 S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab.  X=no date on sample","Ordovician-Cambrian Systems","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-113366845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01402046","Sample-Routine","Water","Surface Water","2014-06-11","09:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02207435",null,"A-1680209 4 Drops HCl",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98396156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY933/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01500422","Sample-Routine","Water","Groundwater","2014-12-04","09:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361100119010001",null,"L-3390078 7th GCV is actually a PHARM,paa,12/5/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104659895","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-12-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404278","Sample-Routine","Water","Groundwater","2014-08-13","10:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363618121381901",null,"L-2300123 Received August 15, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-105558893","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01400502","Sample-Routine","Water","Groundwater","2014-08-18","09:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Michigan Water Science Center","USGS-461500085550001",null,"L-2320070 Received August 19, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Other","NWIS-98954097","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01401127","Sample-Routine","Water","Groundwater","2014-08-26","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392929077530202",null,"L-2400141 Received August 27,2014  Received August 27, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-99284451","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01401662","Sample-Routine","Water","Groundwater","2014-09-03","14:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-384902090451201",null,"A-2470115 Pest Sample  Environmental Sample: VOCs have 3 drops HCl in each vial  GW Radchem - (6) 1L bottles, preserved with 2mL NA  Radon sample collected @ 1505  University of Miami Tritium Laboratory  1 LITER BOTTLE FOR TRITIUM ANALYSIS",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-99209953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-06","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402327","Sample-Routine","Water","Groundwater","2014-07-10","09:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-443921089152001",null,"L-1950012 Received July 11, 2014",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113370647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402933","Sample-Routine","Water","Groundwater","2014-05-15","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-332011116534301",null,"L-1390212 Received May 17, 2014  ASR missing mandatory field alk, paa   alk added per NWQL LC2109, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112106990","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-30","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01401641","Sample-Routine","Water","Surface Water","2014-05-16","08:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02336120",null,"A-1400253 2002943  10 min offset",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97962970","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY1086/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404630","Sample-Routine","Water","Groundwater","2014-09-15","11:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-383916122473501",null,"L-2610121 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106888016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01403521","Sample-Routine","Water","Groundwater","2014-08-27","11:00:00","MDT",{"$nulls":13},"USGS - Colorado Water Science Center","USGS-360027106063401",null,"L-2410097 Samples were received chilled at the WHOI lab.","Santa Fe Group","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-99201965","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01400646","Sample-Routine","Water","Groundwater","2014-09-09","10:00:00","EST",{"$nulls":4},200,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-341249081320100",null,"L-2530014 proj acct chg per F.Falls, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-99256420","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401474","Sample-Routine","Water","Groundwater","2014-08-26","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362336079270001",null,"L-2460143 Received August 29, 2014  Proposal corrected, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99190780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-05","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MA","USGS Massachusetts Water Science Center","nwisma.01.01401000","Sample-Routine","Water","Groundwater","2014-07-15","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-414859072185801",null,"L-1970078 ASR recvd from Miami lab 10/1/14, paa  Samples were received chilled at the WHOI lab.","Stratified Deposits, Undifferentiated","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98777022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01401179","Sample-Routine","Water","Surface Water","2014-04-17","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02336410",null,"A-1120107 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97680305","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY1194/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402565","Sample-Routine","Water","Groundwater","2014-04-25","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-325122116562101",null,"L-1180173 RECEIVED APRIL 25, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112104378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01400468","Sample-Routine","Water","Groundwater","2014-07-21","12:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-321245091495501",null,"L-2030134 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-98765004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404086","Sample-Routine","Water","Groundwater","2014-08-06","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700121580001",null,"A-2200034 DROPS OF VOC ACID= 3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106883755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401183","Sample-Routine","Water","Surface Water","2014-06-11","08:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02146470",null,"L-1690040 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98464836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$f":"BY1282/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01400480","Sample-Routine","Water","Groundwater","2014-07-23","11:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-323308091310801",null,"L-2060048 S1792 changed to S1979 by TAL,paa  Samples were received chilled at the WHOI lab.  end date & time added per Roland, paa, 7/25/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98765511","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402598","Sample-Routine","Water","Groundwater","2014-07-22","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444829089161301",null,"L-2050054 Received July 23, 2014",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113377588","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01503555","Sample-Routine","Water","Groundwater","2015-07-16","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314348094421401",null,"L-1980183 Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-101354024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-07-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01501719","Quality Control Sample-Field Replicate","Water","Groundwater","2015-01-13","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361700119340001",null,"L-0140025 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112108390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-01-23","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01501441","Quality Control Sample-Field Replicate","Water","Groundwater","2015-05-14","11:05:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-382915100544201",null,"L-1350149 X=no station id on PHARM or PEST",null,"Stable, normal stage","Routine sample",null,null,8040,"USGS parameter code 82398","Spigot",null,"Jet pump","NWIS-100825791","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-21","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500742","Sample-Routine","Water","Groundwater","2015-04-16","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-292420081084001",null,"L-1100037 Received April 17, 2015  H2S - Yes Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-109648933","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-26","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01503101","Sample-Routine","Water","Groundwater","2015-09-02","16:10:00","PDT",{"$nulls":4},70.5,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-462824119140801",null,"L-2530076 FED EX LATE DELIVERY",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101838290","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-16","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500794","Sample-Routine","Water","Groundwater","2015-04-28","13:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-271752081214001",null,"L-1190110 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109653263","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600557","Quality Control Sample-Field Replicate","Water","Groundwater","2015-12-09","13:20:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390300121030001",null,"A-3450174 DROPS OF VOC ACID=5",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112116069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503724","Quality Control Sample-Field Replicate","Water","Groundwater","2015-04-27","12:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-355447119250001",null,"A-1190049 DROPS OF VOC ACID = 3",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-104668921","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-02","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600018","Sample-Routine","Water","Groundwater","2015-10-07","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-410800122180001",null,"L-2860037 Received October 09, 2015  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106933995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-10-17","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01504674","Sample-Routine","Water","Groundwater","2015-08-27","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-304246096521201",null,"L-2400164 Changed Station ID to current per P. Ging. JPC 8/29/16  Samples were received chilled at the WHOI lab. Changed Station ID to current per P. Ging. JPC 8/29/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-101831047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600559","Sample-Routine","Water","Groundwater","2015-12-08","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391300120590001",null,"A-3430037 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112116437","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-11","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500792","Sample-Routine","Water","Groundwater","2015-04-23","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-264460080406001",null,"L-1170058 Received April 24, 2015  1792 switched to 1979 due to high solids  H2S =Yes 76ug/L Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-109652028","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503041","Sample-Routine","Water","Groundwater","2015-04-01","10:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361400119460001",null,"L-0920079 ASR missing WSC contact, paa  Samples were received chilled at the WHOI lab.  Smdugan added, S1792 changed to S1979 by ALS, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104666390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600595","Sample-Routine","Water","Groundwater","2015-12-17","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392400120570001",null,"A-3520032 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112117167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-28","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500783","Sample-Routine","Water","Groundwater","2015-08-11","16:00:00","CDT",{"$nulls":4},11.5,"feet",null,14.5,"feet",19.5,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-384646090375501",null,"A-2240121 Alternate contact-Kelly Warner(klwarner)/217-328-09727   drops HCL for VOC  Alternate contact - Kelly Warner, klwarner@usgs.gov 217-328-9725. Acidified with HNO3. Acidified with HNO3. RADCHEM - acidified HNO3","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101521623","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-15","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503313","Sample-Routine","Water","Groundwater","2015-04-09","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-354800119060001",null,"L-1000023 ASR missing WSC contact,paa  Samples were received chilled at the WHOI lab.  rhkent added, paa   1792 changed to 1679 due to re-prep required by low LCS--Recount outside holding time,per Mullin.  KB 6/30/15",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-104667466","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500568","Sample-Routine","Water","Surface Water","2015-06-22","13:30:00","CST",{"$nulls":13},"USGS - Illinois Water Science Center","USGS-05537000",null,"A-1770033 Attn: Mississippi River Study.",null,"Rising stage","Routine sample",null,null,15,"USGS parameter code 82398","10 or more equal width verticals, equal non-iso transit rate limited by velocity",null,"Weighted-bottle sampler","NWIS-101100449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$f":"BY1632/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500976","Sample-Routine","Water","Groundwater","2015-06-29","12:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-301930082585001",null,"L-1810103 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109657592","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-07-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01505446","Sample-Routine","Water","Groundwater","2015-09-14","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373600121170001",null,"L-2600060 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106932931","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-24","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500975","Sample-Routine","Water","Surface Water","2015-08-26","13:00:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05543500",{"$nulls":3},"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-101745018","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$f":"BY1695/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500413","Sample-Routine","Water","Surface Water","2015-05-07","10:30:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05541510",null,"L-1320087 X=no btl types on GCC, GCV, OXW, PEST, PHARM and TOC, no schedule or lab codes on btls   Received May 09, 2015..  Emailed WSC contact, missing proposal # for LC 9030,3406,9031,4440, & 8099, ACW, 5/13/15 Added proposal # CL15023, ACW, 5/19/15",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-100743136","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-14","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$f":"BY1720/2","v":0.04},"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01500190","Sample-Routine","Water","Groundwater","2015-06-15","13:00:00","EST",{"$nulls":14},"USGS-324505081145100",null,"L-1670065 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-101043504","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-20","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01501438","Sample-Routine","Water","Groundwater","2015-05-14","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-382915100544201",null,"L-1350064 Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,8040,"USGS parameter code 82398","Spigot",null,"Jet pump","NWIS-100824600","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-16","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600453","Sample-Routine","Water","Groundwater","2015-11-30","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361801119380001",null,"A-3360131 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106940150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-08","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01500568","Quality Control Sample-Field Replicate","Water","Groundwater","2015-05-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-425400070545401",null,"L-1400121 Added proposal number CL15NAWNH,and program/project code GWMSA per Flanagan,ACW,5/20/15  Samples were received chilled at the WHOI lab.","Bedrock","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-100718443","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-22","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601397","Sample-Routine","Water","Groundwater","2016-07-20","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-471928118412501",null,"L-2030129 X=no time on DOC & GCVs  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105284288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01603038","Sample-Routine","Water","Groundwater","2016-08-03","12:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431037090043401",null,"L-2439605 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-113537035","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701153","Sample-Routine","Water","Groundwater","2016-11-30","15:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325527097305701",null,"L-3360010 Samples were received chilled at the WHOI lab.  Schedule 1792 changed to 1979 due to solids",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106530340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01600678","Quality Control Sample-Field Replicate","Water","Groundwater","2016-05-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-425400070545401",null,"L-1450069 Samples were received chilled at the WHOI lab.","Bedrock","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103900426","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01700832","Sample-Routine","Water","Groundwater","2016-12-06","12:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365600118140001",null,"L-3440100 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-109454110","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01601988","Sample-Routine","Water","Groundwater","2016-01-26","12:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-282009099044001",null,"L-0270030 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103547870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-01-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01602333","Sample-Routine","Water","Groundwater","2016-03-15","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392800121150001",null,"L-0770037 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112122338","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01603730","Sample-Routine","Water","Groundwater","2016-06-16","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","TX001-352134101324007",null,"L-1690154 Changed Station ID to current per P. Ging. JPC 8/29/16  Samples were received chilled at the WHOI lab. Changed Station ID to current per P. Ging. JPC 8/29/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105054980","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01600217","Sample-Routine","Water","Groundwater","2016-07-05","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392506119462201",null,"L-1890024 FED EX LATE DELIVERY  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105138590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01602049","Sample-Routine","Water","Groundwater","2016-02-09","15:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-285144097443401",null,"L-0410075 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103564480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-19","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01603740","Sample-Routine","Water","Groundwater","2016-05-25","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","TX001-341237102454818",null,"L-1470074 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105059384","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701155","Sample-Routine","Water","Groundwater","2016-11-28","12:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320933099095201",null,"L-3340032 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106531590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-11-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01604709","Sample-Routine","Water","Groundwater","2016-08-01","12:30:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351347106370301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105514161","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01601401","Sample-Routine","Water","Groundwater","2016-01-14","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-281546099234601",null,"L-0150099 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103269301","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-01-20","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01603924","Sample-Routine","Water","Groundwater","2016-05-16","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-351500118370001",null,"L-1410115 Time and date on RU & FU 1600  05102016  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108900390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01603891","Sample-Routine","Water","Groundwater","2016-05-17","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371200119400001",null,"L-1440037 X=FU has an FA label. Ok to login warm per T.Mathany Chilled containers received warm at 18.6  Degrees C  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108898579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-25","sample was warm when receivedsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01604119","Sample-Routine","Water","Groundwater","2016-05-24","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392700120390001",null,"L-1470019 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112125494","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601368","Sample-Routine","Water","Groundwater","2016-06-28","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-464016119543901",null,"L-1820169 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105141450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01605762","Quality Control Sample-Field Replicate","Water","Groundwater","2016-08-08","09:50:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391523120422401",null,"L-2240035 FED EX LATE DELIVERY  No tape, cap loose - no leak or loss of smaple Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-112127357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01601538","Sample-Routine","Water","Groundwater","2016-08-30","09:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-261537080141601",null,"L-2440030 Samples were received chilled at the WHOI lab. Result 77035, rejected on 12/21/21, because a national-scale QC evaluation for groundwater indicated that contamination bias likely resulted in relatively common detections taht do not represent environmental conditions.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109261196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701147","Sample-Routine","Water","Groundwater","2016-12-12","12:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333826097213601",null,"L-3480090 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106528456","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701159","Sample-Routine","Water","Groundwater","2016-11-16","10:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300358099100901",null,"L-3220058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106536719","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-11-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01606334","Sample-Routine","Water","Groundwater","2016-09-12","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384617120460001",null,"L-2590083 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112129960","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601415","Sample-Routine","Water","Groundwater","2016-07-27","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-472756117373001",null,"L-2158705 Samples were received chilled at the WHOI lab.  Added user code WA. 8/4/2016 mec",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105338489","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01700212","Sample-Routine","Water","Groundwater","2016-11-16","12:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-485930122431001",null,"L-3230003 X=received #1 of 4437 vials broken.  Added Schedules 4436 and 4437 per Huffman. 11/21/2016 mec  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-106271902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-11-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601613","Sample-Routine","Water","Groundwater","2016-02-02","09:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390500121000001",null,"L-0340045 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112120118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601669","Sample-Routine","Water","Groundwater","2016-02-10","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374109121000101",null,"L-0430204 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106942769","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-19","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01601516","Sample-Routine","Water","Groundwater","2016-06-13","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-254934080250401",null,"L-2608734 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109248816","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OR","USGS Oregon Water Science Center","nwisor.01.01600402","Sample-Routine","Water","Groundwater","2016-07-13","09:00:00","PDT",{"$nulls":4},300,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452550117152001",null,"L-1960139 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Other","NWIS-110441435","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01701322","Sample-Routine","Water","Groundwater","2017-01-19","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385801121055801",null,"L-0200032 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112138350","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-01-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800068","Sample-Routine","Water","Groundwater","2017-10-19","09:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382600121305501",null,"L-2930055 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110972986","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700553","Sample-Routine","Water","Groundwater","2017-08-01","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392853075005801",null,"L-2349602 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108379633","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703760","Sample-Routine","Water","Groundwater","2017-08-08","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305904103534001",null,"L-2210182 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108588995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01701317","Sample-Routine","Water","Groundwater","2017-08-10","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414540075453201",null,"L-2230184 WHOI comment: \"Bottle broken but sample intact.\" KB 8/14/17 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108469303","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01702592","Sample-Routine","Water","Groundwater","2017-08-02","09:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-421130076254201",null,"L-2150079 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-108698032","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01702797","Sample-Routine","Water","Groundwater","2017-09-27","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424631073391401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-109098848","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707839","Quality Control Sample-Field Replicate","Water","Groundwater","2017-09-20","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385200120000001",null,"L-2650153 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115691020","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01702927","Sample-Routine","Water","Groundwater","2017-02-22","12:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-334700116100001",null,"L-1388703 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-110780380","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-02-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707311","Sample-Routine","Water","Groundwater","2017-08-24","13:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382404121250201",null,"L-2370018 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110968136","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01701323","Sample-Routine","Water","Groundwater","2017-08-14","13:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-415827075560001",null,"L-2270214 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108511778","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707677","Sample-Routine","Water","Groundwater","2017-09-12","14:00:00","PDT",{"$nulls":4},160,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-384455121292101",null,"L-2560095 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110970496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01702158","Sample-Routine","Water","Groundwater","2017-04-10","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305624097321101",null,"L-1010241 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-107601248","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-04-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703756","Sample-Routine","Water","Groundwater","2017-06-07","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302646099481501",null,"L-1590298 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108587112","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701579","Sample-Routine","Water","Groundwater","2017-03-07","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-291943099163301",null,"L-0670023 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106974659","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-03-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01706099","Sample-Routine","Water","Groundwater","2017-06-28","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-342123119024201",null,"L-1810267 X=no date, time, or STA ID on GCC  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115683481","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700639","Sample-Routine","Water","Groundwater","2017-08-21","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394604075003601",null,"L-2360059 X=DOC not received.  Deleted LC2612. 8/25/2017 mec  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-108554127","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707116","Sample-Routine","Water","Groundwater","2017-08-07","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381731121183001",null,"L-2210049 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-110967723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800670","Sample-Routine","Water","Groundwater","2017-12-18","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-423523076220902",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-109375376","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-12-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01700138","Sample-Routine","Water","Groundwater","2017-08-16","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351113089513401",null,"L-2300038 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-108568946","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CT","USGS Connecticut Water Science Center","nwisma.01.01700616","Sample-Routine","Water","Groundwater","2017-04-10","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-414245072333901",null,"L-1020045 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Jet pump","NWIS-107305888","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-04-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700461","Sample-Routine","Water","Groundwater","2017-06-19","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394255075030401",null,"L-2059601 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107897603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703761","Sample-Routine","Water","Groundwater","2017-06-28","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303418100382101",null,"L-1800327 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Line-shaft turbine pump","NWIS-108595352","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01701204","Sample-Routine","Water","Groundwater","2017-07-19","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381034109274501",null,"L-2010187 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible positive-pressure pump","NWIS-108424763","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800041","Sample-Routine","Water","Groundwater","2017-10-12","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-324400114380001",null,"L-2860114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115691538","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-19",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700462","Sample-Routine","Water","Groundwater","2017-06-21","09:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394321075015701",null,"L-2059602 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107897803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700658","Sample-Routine","Water","Groundwater","2017-08-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394340075012701",null,"L-2909608 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-108621234","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01800155","Sample-Routine","Water","Groundwater","2018-03-28","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332918112283301",null,"L-0880139 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110563647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01801082","Sample-Routine","Water","Groundwater","2018-06-19","09:20:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-395012094540101",null,"L-1710072 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8030,"USGS parameter code 82398","Grab sample at water-supply tap",null,"Submersible gear pump","NWIS-111193961","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01800927","Sample-Routine","Water","Groundwater","2018-09-17","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393035074533601",null,"L-2610069 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible centrifugal pump","NWIS-111828227","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800726","Sample-Routine","Water","Groundwater","2018-07-19","13:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-475427103361401",null,"L-2198712 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111319515","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-07-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01805847","Sample-Routine","Water","Groundwater","2018-09-12","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363500118140001",null,"L-2570171 Add District Contact RHKENT to ASR.  KMS, 9/17/18  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-118317003","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01801656","Sample-Routine","Water","Groundwater","2018-03-13","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-293745098162001",null,"L-0730036 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110505318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01900247","Sample-Routine","Water","Groundwater","2018-11-20","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-434803075402901",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-115483496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802025","Sample-Routine","Water","Groundwater","2018-02-26","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345455117052601",null,"L-0600042 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116128032","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01800229","Sample-Routine","Water","Groundwater","2018-06-27","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-452350093510301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111216564","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01801150","Sample-Routine","Water","Groundwater","2018-07-16","10:00:00","CDT",{"$nulls":4},18.2,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-372329097105501",null,"L-1980207 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-111289558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-07-19",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01900338","Sample-Routine","Water","Groundwater","2018-10-23","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340742116053201",null,"L-2990163 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-118324607","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802022","Sample-Routine","Water","Groundwater","2018-02-27","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-344856116373901",null,"L-0600048 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116127619","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01900033","Sample-Routine","Water","Groundwater","2018-10-03","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-440207075402801",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-112069783","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-10-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802942","Sample-Routine","Water","Groundwater","2018-04-05","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370145121560101",null,"L-1638708 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115702173","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-04-27","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802023","Quality Control Sample-Field Replicate","Water","Groundwater","2018-02-27","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-344927116394101",null,"L-0600044 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115697800","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01801534","Sample-Routine","Water","Groundwater","2018-01-29","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345245116435801",null,"L-0330077 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116125556","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-02-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01803340","Sample-Routine","Water","Groundwater","2018-04-16","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-343953118041901",null,"L-1100101 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115954750","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-04-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01800232","Sample-Routine","Water","Groundwater","2018-06-26","10:30:00","CDT",{"$nulls":4},4.3,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-452036093423701",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111217532","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01805759","Sample-Routine","Water","Groundwater","2018-08-29","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-375100119560001",null,"L-2430110 X=time on samples is 1500, no sta id, date or time on GCC.  Added project chief RHKENT. 9/5/2018 mec  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-118319878","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01900104","Sample-Routine","Water","Groundwater","2018-10-30","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-412418074244202",null,"L-3068501 Updated SID/SID Name from 412309074264203/O 222 per D. Jensen. JPC 5/21/19  Updated SID from 412309074264203 per K. Colella. JPC 11/8/18",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-112211703","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01902411","Sample-Routine","Water","Groundwater","2019-09-24","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310934081404801",null,"L-2758702 Samples were received chilled at the WHOI lab. L-2680141 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117842931","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906976","Quality Control Sample-Field Replicate","Water","Groundwater","2019-09-25","13:50:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380337121301001",null,"L-2700098 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124193054","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906863","Quality Control Sample-Field Replicate","Water","Groundwater","2019-09-10","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374824120503001",null,"L-2540074 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118732780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01902574","Sample-Routine","Water","Groundwater","2019-09-11","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USEPA-403132080374501",null,"L-2550043 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117750949","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01902529","Sample-Routine","Water","Groundwater","2019-09-04","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USEPA-395803081593401",null,"L-2490059 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117686292","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902080","Sample-Routine","Water","Groundwater","2019-06-20","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420134070432301",null,"L-1728502 X = Time on RU looks like 2100.",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116954541","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-06-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01901186","Sample-Routine","Water","Groundwater","2019-04-04","15:00:00","EDT",{"$nulls":4},8,"feet",null,7.92,"feet",12.92,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-262854081241301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-117396044","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-04-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01902596","Sample-Routine","Water","Groundwater","2019-02-28","09:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401754122161601",null,"L-0630002 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118297980","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-03-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01902599","Quality Control Sample-Field Replicate","Water","Groundwater","2019-02-26","12:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401501122285301",null,"L-0590004 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118298825","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-03-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906468","Quality Control Sample-Field Replicate","Water","Groundwater","2019-08-19","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380434120544601",null,"L-2330139 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118734985","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01903540","Sample-Routine","Water","Groundwater","2019-03-26","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-403032122193301",null,"L-0880115 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118302810","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-04-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902643","Sample-Routine","Water","Groundwater","2019-08-08","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-423713070481301",null,"L-2250079 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117610655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01901943","Sample-Routine","Water","Groundwater","2019-07-15","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-433320073153401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-117195965","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000381","Sample-Routine","Water","Groundwater","2019-10-30","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-263000081390001",null,"L-3040027 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118426130","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IN","USGS Indiana Water Science Center","nwisin.01.01901101","Sample-Routine","Water","Groundwater","2019-09-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385053084485901",null,"L-2630105 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-118209563","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906320","Sample-Routine","Water","Groundwater","2019-08-06","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374909121110101",null,"L-2190044 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118737827","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-10",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01903538","Sample-Routine","Water","Groundwater","2019-03-27","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-402348122112701",null,"L-0880117 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118302241","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-04-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000375","Sample-Routine","Water","Groundwater","2019-10-29","17:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-262500081430001",null,"L-3030196 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118424870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IN","USGS Indiana Water Science Center","nwisin.01.01901088","Sample-Routine","Water","Groundwater","2019-08-21","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375327087030301",null,"MM-57883A",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Mulitple samplers used","NWIS-117753455","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906315","Sample-Routine","Water","Groundwater","2019-08-08","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380919121043901",null,"L-2210101 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118739411","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01901608","Sample-Routine","Water","Groundwater","2019-02-05","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700120220001",null,"L-0390030 Received 3/19/2019 chilled. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118034474","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-02-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.02100016","Sample-Routine","Water","Groundwater","2020-10-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-400642083441601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-119904717","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-10-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100722","Sample-Routine","Water","Groundwater","2020-12-03","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374240120432601",null,"L-3390097 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122456079","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-12-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001510","Quality Control Sample-Field Replicate","Water","Groundwater","2020-01-15","09:50:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-335727116524701",null,"L-0170105 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120719027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-02-01","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001725","Sample-Routine","Water","Groundwater","2020-07-23","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-444454075075401",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119361877","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001992","Sample-Routine","Water","Groundwater","2020-02-24","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-334031116151201",null,"L-0590103 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120713674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-03-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003425","Sample-Routine","Water","Groundwater","2020-07-22","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334350117553201",null,"L-2100022 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-119368581","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Hold time parameters were exceeded during the collection to analysis phase of sample processing.",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100516","Sample-Routine","Water","Groundwater","2020-11-16","14:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-405600123370001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122575031","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-11-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02100358","Sample-Routine","Water","Groundwater","2020-10-29","10:00:00","EDT",{"$nulls":4},13.5,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-261525080165101",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120385035","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-10-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001860","Sample-Routine","Water","Groundwater","2020-08-03","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-420125074474901",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119547118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001781","Sample-Routine","Water","Groundwater","2020-08-17","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-415601074544901",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119479317","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003635","Sample-Routine","Water","Groundwater","2020-07-21","10:15:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380948121360901",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-120694374","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001736","Sample-Routine","Water","Groundwater","2020-07-27","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425825077422201",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119400094","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003639","Sample-Routine","Water","Groundwater","2020-07-15","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341400116510001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120695609","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100024","Sample-Routine","Water","Groundwater","2020-10-26","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",100,"feet",95,"feet",null,null,"U.S. Geological Survey","USGS-301618092035701",null,"L-3010127 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Jet pump","NWIS-119955663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-10-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02000346","Sample-Routine","Water","Groundwater","2020-07-29","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",140,"feet",150,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305020093003001",null,"L-2120201 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Jet pump","NWIS-119388926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003821","Sample-Routine","Water","Groundwater","2020-08-17","10:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-360000120540001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-121372371","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02104660","Sample-Routine","Water","Groundwater","2021-07-14","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390900122030001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-125820083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02103882","Sample-Routine","Water","Groundwater","2021-06-08","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-335710118211801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-125826372","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102573","Sample-Routine","Water","Groundwater","2021-03-31","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-352900119320001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-122875357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-04-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100260","Sample-Routine","Water","Groundwater","2021-06-15","14:00:00","CDT",{"$nulls":4},45,"feet",null,46,"feet",56,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-301234092012401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121294431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-23","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101968","Sample-Routine","Water","Groundwater","2021-02-24","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-372746120443601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-122467130","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-03-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102114","Sample-Routine","Water","Groundwater","2021-03-08","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373647120273801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122468715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-03-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101909","Sample-Routine","Water","Groundwater","2021-02-16","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-360945119200001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-122824775","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100263","Sample-Routine","Water","Groundwater","2021-06-16","15:00:00","CDT",{"$nulls":4},45,"feet",null,47,"feet",67,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-300932092003801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121295109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-25","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101866","Sample-Routine","Water","Groundwater","2021-07-29","09:15:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-423200078250001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-121686858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-08-04","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101333","Sample-Routine","Water","Groundwater","2021-01-12","13:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392600121100001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122737291","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-01-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.02100348","Sample-Routine","Water","Groundwater","2021-05-20","09:00:00","CST",{"$nulls":4},20,"feet",null,23.08,"feet",28.08,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-425913088133801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122722743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-05-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101595","Quality Control Sample-Field Replicate","Water","Groundwater","2021-01-27","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371832120231201",null,"L-0320024 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-122463327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101658","Sample-Routine","Water","Groundwater","2021-02-09","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371555120285101",null,"L-0530056 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122464276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Hold time parameters were exceeded during the collection to analysis phase of sample processing.",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-24","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101907","Sample-Routine","Water","Groundwater","2021-02-17","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-362128119390001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-122824150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101966","Sample-Routine","Water","Groundwater","2021-09-13","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424235078323101",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-121900574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100226","Sample-Routine","Water","Groundwater","2021-05-26","15:00:00","CDT",{"$nulls":4},38,"feet",null,41,"feet",51,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-300824091593201",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121167201","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-05-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02202669","Sample-Routine","Water","Groundwater","2022-03-15","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-353024119213401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125814561","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-03-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.02200593","Sample-Routine","Water","Groundwater","2022-08-31","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384645076044401",{"$nulls":3},"Not determined","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Suction pump","NWIS-124281604","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02205688","Sample-Routine","Water","Groundwater","2022-08-29","12:30:00","PDT",{"$nulls":14},"USGS-370625121370401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125806006","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.02300377","Sample-Routine","Water","Groundwater","2022-10-18","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303809097404701",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124641880","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-10-27","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201195","Sample-Routine","Water","Groundwater","2022-07-28","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424544076371801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-124060406","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-02","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02201622","Sample-Routine","Water","Groundwater","2022-06-28","16:00:00","EDT",{"$nulls":6},"Below land-surface datum",162.17,"feet",232.92,"feet",null,null,"U.S. Geological Survey-Water Resources Discipline","USGS-332137081581301",null,null,"Midville Aquifer System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124096086","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.02200022","Sample-Routine","Water","Groundwater","2022-03-07","13:00:00","CST",{"$nulls":4},17,"feet",null,14,"feet",24,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344124086531401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-123779311","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-03-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.02200511","Sample-Routine","Water","Groundwater","2022-04-04","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365751076363001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-123455480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-04-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203906","Sample-Routine","Water","Groundwater","2022-05-17","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384814123044001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125236430","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-05-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02204512","Sample-Routine","Water","Groundwater","2022-06-07","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381344122202901",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125239703","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201194","Sample-Routine","Water","Groundwater","2022-07-27","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425855075512201",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-124060123","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-02","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02205771","Sample-Routine","Water","Groundwater","2022-09-13","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370126121301001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125803661","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02300256","Sample-Routine","Water","Groundwater","2022-10-25","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-333130114394001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-125801157","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-11-02","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201423","Sample-Routine","Water","Groundwater","2022-08-09","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-434343074033101",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124116756","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201653","Quality Control Sample-Field Replicate","Water","Groundwater","2022-08-24","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431001076243501",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124616989","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203914","Sample-Routine","Water","Groundwater","2022-05-25","11:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381448122542001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125236208","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.02301802","Sample-Routine","Water","Groundwater","2023-08-02","12:30:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-402119075112801",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-126006339","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-12","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.02300581","Sample-Routine","Water","Groundwater","2023-08-22","10:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395521088344201",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-126221076","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.02301769","Sample-Routine","Water","Groundwater","2023-07-26","10:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401405075275101",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-125970134","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-04","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW02-VP-D001-052004-0","Sample","Air","Ambient Air","2004-05-20","15:40:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW02",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047849995.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-05-24",{"$nulls":3},5.6,"ppb",{"$nulls":4},"STORET"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW04-VP-D004-052004-0","Sample","Air","Ambient Air","2004-05-23","10:54:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW04",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047851492.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-05-27",{"$nulls":3},6.8,"ppb",{"$nulls":4},"STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-95543R-gwdb","Sample-Routine","Water","Groundwater","2011-10-28","09:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-77503","CLEAN HARBORS AZ CH-4",{"$nulls":4},33.4421758,-112.0904453,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-492536578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2011-11-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-95543R-gwdb/results/492536578/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2015-12-04T11:52:06","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120443R-gwdb","Sample-Other","Water","Groundwater","2013-08-01","15:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490947484",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-04",{"$nulls":8},"2015-11-30T18:43:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120268R-gwdb","Sample-Other","Water","Groundwater","2013-08-01","12:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490859446",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-04",{"$nulls":8},"2015-11-30T17:54:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120359R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","07:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120359R-gwdb/results/490802011/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T17:14:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120279.CHEM","Sample-Routine","Other",null,"2013-08-01","11:20:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-53578",64410,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725051519","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120279.CHEM/results/725051519/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2018-05-10T17:39:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120314.CHEM","Sample-Routine","Other",null,"2013-08-01","02:05:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-52553",62913,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.52445,-112.0817647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725053568","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120314.CHEM/results/725053568/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2018-05-10T17:39:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120442.CHEM","Sample-Routine","Other",null,"2013-08-01","02:35:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-58790",79323,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5244922,-112.0817217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725056945","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120442.CHEM/results/725056945/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2018-05-10T17:40:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132031-gwdb","Sample-Routine","Water","Groundwater","2013-09-11","12:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490893729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-15",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132031-gwdb/results/490893729/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:19:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132025-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","13:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79231","ADEQ MW-111",{"$nulls":4},32.2457594,-109.8359936,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962368","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132025-gwdb/results/490962368/resdetectqntlmts","Lower Reporting Limit",0.02,"mg/L",{"$nulls":3},"2015-11-30T18:49:39","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120478R-gwdb","Sample-Other","Water","Groundwater","2013-10-30","11:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769095",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-11-03",{"$nulls":8},"2015-11-30T16:47:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120333R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","09:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490942682","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-01-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120333R-gwdb/results/490942682/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:41:31","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122435-gwdb","Sample-Routine","Water","Groundwater","2014-09-24","11:44:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490880201","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122435-gwdb/results/490880201/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:10:08","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122139-gwdb","Sample-Routine","Water","Groundwater","2014-03-10","13:58:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64047","COP MW-48",{"$nulls":4},33.5008917,-112.1459333,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490875006",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-14",{"$nulls":8},"2015-11-30T18:05:31","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122147-gwdb","Sample-Routine","Water","Groundwater","2014-03-11","10:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-59282","WCP-72M",{"$nulls":4},33.4994497,-112.1465058,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490871679",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-14",{"$nulls":8},"2015-11-30T18:02:07","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121776-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","07:37:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490946274","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121776-gwdb/results/490946274/resdetectqntlmts","Lower Reporting Limit",0.04,"mg/L",{"$nulls":3},"2015-11-30T18:42:38","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132368-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","12:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-57556","YELLOW CAB RW-1",{"$nulls":4},32.2267939,-110.9675289,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882980","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132368-gwdb/results/490882980/resdetectqntlmts","Lower Reporting Limit",0.02,"mg/L",{"$nulls":3},"2015-11-30T18:12:54","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122418-gwdb","Sample-Routine","Water","Groundwater","2014-05-20","12:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79264","ADEQ MW-104",{"$nulls":4},32.2674414,-109.8470308,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017719","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122418-gwdb/results/491017719/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T19:17:37","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122449-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","11:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490877351","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122449-gwdb/results/490877351/resdetectqntlmts","Lower Reporting Limit",0.2,"mg/L",{"$nulls":3},"2015-11-30T18:07:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122128-gwdb","Sample-Routine","Water","Groundwater","2014-03-06","09:40:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-59417","WCP-78",{"$nulls":4},33.5025417,-112.1515417,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491015285",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-12",{"$nulls":8},"2015-11-30T19:16:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122443-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","07:58:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490808223","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122443-gwdb/results/490808223/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T17:19:01","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132478-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","15:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490889746","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132478-gwdb/results/490889746/resdetectqntlmts","Lower Reporting Limit",0.2,"mg/L",{"$nulls":3},"2015-11-30T18:17:17","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122414-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","14:48:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79262","ADEQ MW-102",{"$nulls":4},32.26686,-109.8468753,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490957723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122414-gwdb/results/490957723/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:47:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148945-gwdb","Sample-Other","Water","Groundwater","2015-10-22","16:04:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65186","MW-203M",{"$nulls":4},33.4799944,-112.1385917,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552065549","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148945-gwdb/results/552065549/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T02:28:45","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148929-gwdb","Sample-Other","Water","Groundwater","2015-10-23","14:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-60383","WCP-204",{"$nulls":4},33.4819272,-112.1311575,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551993247","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148929-gwdb/results/551993247/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T01:47:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150795-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","14:10:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79949","THOMPSON TDI-20",{"$nulls":4},34.9024192,-110.1634028,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552046911","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-11",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150795-gwdb/results/552046911/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2016-05-12T02:20:42","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150784-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","12:00:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79941","THOMPSON TDI-1",{"$nulls":4},34.9025122,-110.1633353,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552064700","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150784-gwdb/results/552064700/resdetectqntlmts","Lower Reporting Limit",10,"ug/L",{"$nulls":3},"2016-05-12T02:28:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148329-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","12:59:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79226","ADEQ MW-106",{"$nulls":4},32.2460858,-109.8359989,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552135625","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148329-gwdb/results/552135625/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T02:58:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146182-gwdb","Sample-Routine","Water","Groundwater","2015-03-16","13:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-58229","IRA-9",{"$nulls":4},32.27998,-111.0031697,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552150379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-20",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146182-gwdb/results/552150379/resdetectqntlmts","Method Detection Level",2,"ug/L",{"$nulls":3},"2016-05-12T03:08:36","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144200-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","12:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552007178","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144200-gwdb/results/552007178/resdetectqntlmts","Lower Reporting Limit",0.05,"mg/L",{"$nulls":3},"2016-05-12T01:56:07","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148826-gwdb","Sample-Routine","Water","Groundwater","2015-09-22","09:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-80426","KENGLA WELL 3",{"$nulls":4},34.1506231,-109.9747219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552170565","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-09-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148826-gwdb/results/552170565/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2016-05-12T03:14:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148939-gwdb","Sample-Other","Water","Groundwater","2015-10-22","11:47:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57159","WOC MW-06M",{"$nulls":4},33.4839803,-112.1425672,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552171293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148939-gwdb/results/552171293/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T03:14:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148979-gwdb","Sample-Routine","Water","Groundwater","2015-11-20","08:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552175226","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148979-gwdb/results/552175226/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T03:15:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146160-gwdb","Sample-Routine","Water","Groundwater","2015-03-10","13:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57685","IRA-4",{"$nulls":4},32.2709558,-111.0032325,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551973134","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146160-gwdb/results/551973134/resdetectqntlmts","Method Detection Level",2,"ug/L",{"$nulls":3},"2016-05-12T01:29:46","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146154-gwdb","Sample-Routine","Water","Groundwater","2015-03-16","10:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-36092","VILLA CAPRI  WELL",{"$nulls":4},32.2928333,-111.0141389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552157751","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146154-gwdb/results/552157751/resdetectqntlmts","Method Detection Level",2,"ug/L",{"$nulls":3},"2016-05-12T03:11:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147255-gwdb","Sample-Other","Water","Groundwater","2015-03-20","14:12:00","MST",{"$nulls":11},"MISC","MISC",null,"21ARIZ_WQX-59292","HSMW-5U",{"$nulls":4},33.39371,-111.9388003,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551984363","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Xenco Laboratories","2015-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147255-gwdb/results/551984363/resdetectqntlmts","Lower Reporting Limit",5,"ug/L",{"$nulls":3},"2016-05-12T01:39:09","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150946-gwdb","Sample-Routine","Water","Groundwater","2016-03-02","13:25:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80597","MW-6A",{"$nulls":4},33.4928372,-113.1617644,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552020148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150946-gwdb/results/552020148/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2016-05-12T02:03:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155338.CHEM","Sample-Routine","Other",null,"2016-08-09","08:25:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58754",79229,{"$nulls":4},32.2460544,-109.8368444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676181821","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-08-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155338.CHEM/results/676181821/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2017-11-03T10:08:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-150947.CHEM","Sample-Routine","Other",null,"2016-03-03","08:50:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59190",80594,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.492975,-113.1617631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707988435","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-03-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-150947.CHEM/results/707988435/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-03-13T10:39:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155331.CHEM","Sample-Routine","Other",null,"2016-09-14","10:48:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58747",79222,{"$nulls":4},32.2461081,-109.8364322,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676199676","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-09-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155331.CHEM/results/676199676/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2017-11-03T10:11:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155729.CHEM","Sample-Routine","Other",null,"2016-05-03","10:24:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59320",81183,{"$nulls":4},34.5619778,-112.4865694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676260446","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-05-09",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155729.CHEM/results/676260446/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",{"$nulls":3},"2017-11-03T10:24:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156913.CHEM","Sample-Routine","Other",null,"2016-12-06","08:58:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59190",80594,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.492975,-113.1617631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993271","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156913.CHEM/results/707993271/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-03-13T10:41:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156922.CHEM","Sample-Routine","Other",null,"2016-12-05","01:43:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59189",80593,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4927864,-113.1616206,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993964","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156922.CHEM/results/707993964/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-03-13T10:41:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-151704-gwdb","Sample-Other","Water","Groundwater","2016-03-16","14:58:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-58082","WOC MW-201S",{"$nulls":4},33.4803331,-112.136605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552124379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-151704-gwdb/results/552124379/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T02:53:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156041.CHEM","Sample-Routine","Other",null,"2016-09-21","02:01:00","EST",{"$nulls":4},105,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","URS CONSULTANTS","AZDEQ_WPD-58793",79326,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.524588,-112.0825932,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725065646","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX","2016-09-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156041.CHEM/results/725065646/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-05-10T17:42:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-151702.CHEM","Sample-Routine","Water","Groundwater","2016-03-16","11:53:00","EST",{"$nulls":4},155,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-55160",67698,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.4773702,-112.1464663,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-799539083","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-03-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-151702.CHEM/results/799539083/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2019-10-07T11:07:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155321.CHEM","Sample-Routine","Other",null,"2016-09-13","12:00:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58759",79234,{"$nulls":4},32.2459356,-109.8355467,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676198923","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-09-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155321.CHEM/results/676198923/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2017-11-03T10:11:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156252.CHEM","Sample-Routine","Other",null,"2016-10-21","12:20:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","URS CONSULTANTS","AZDEQ_WPD-56983",72800,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5244731,-112.0829683,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725065561","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX","2016-10-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156252.CHEM/results/725065561/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-05-10T17:42:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156916.CHEM","Sample-Routine","Other",null,"2016-12-06","11:46:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59187",80591,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4929192,-113.1616131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993502","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156916.CHEM/results/707993502/resdetectqntlmts","Laboratory Reporting Level",200,"ug/L",{"$nulls":3},"2018-03-13T10:41:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-157559.CHEM","Sample-Routine","Other",null,"2017-02-20","03:12:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59320",81183,{"$nulls":4},34.5619778,-112.4865694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676159780","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2017-02-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-157559.CHEM/results/676159780/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2017-11-03T09:23:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18224.CHEM","Sample-Routine","Water",null,"2017-12-07","11:45:00","EST",{"$nulls":11},9725,"2017-WQARF SAMPLES","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-786710880","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18224.CHEM/results/786710880/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-05-01T10:07:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-157047.CHEM","Sample-Routine","Other",null,"2017-01-30","02:23:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59169",80492,{"$nulls":4},35.1904639,-109.4332189,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676161070","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2017-02-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-157047.CHEM/results/676161070/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2017-11-03T09:23:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18217.CHEM","Sample-Routine","Water",null,"2017-12-03","04:35:00","EST",{"$nulls":11},9725,"2017-WQARF SAMPLES","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-786710362","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18217.CHEM/results/786710362/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-05-01T10:07:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB11228.CHEM","Sample-Routine","Other",null,"2017-10-31","10:55:00","EST",{"$nulls":4},47,"ft",{"$nulls":5},9691,"VRP_0000","CH2M","AZDEQ_WPD-61636",81379,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.939721,-110.302651,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725240834","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"L | QA FLAGS: E8.",null,47,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"XENCO LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB11228.CHEM/results/725240834/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",{"$nulls":3},"2018-05-15T09:02:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB05690.CHEM","Sample-Routine","Other",null,"2017-11-15","11:37:00","EST",{"$nulls":4},145,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725093105","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,145,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB05690.CHEM/results/725093105/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-05-11T10:34:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30380.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2018-11-16","01:25:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903957","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30380.CHEM/results/874903957/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2021-02-05T12:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18668.CHEM","Sample-Routine","Water","Groundwater","2018-11-13","04:05:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184359","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18668.CHEM/results/789184359/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-06-12T10:04:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18669.CHEM","Sample-Routine","Water","Groundwater","2018-11-13","11:30:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183693","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18669.CHEM/results/789183693/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-06-12T10:04:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18667.CHEM","Sample-Routine","Water","Groundwater","2018-11-14","04:05:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61658",81400,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.15071,-109.9747382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18667.CHEM/results/789183915/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-06-12T10:04:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14390.CHEM","Sample-Routine","Other",null,"2018-02-11","01:30:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61859",81549,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.2166806,-114.2024528,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734875908","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14390.CHEM/results/734875908/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2018-09-24T10:46:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14438.CHEM","Sample-Routine","Other",null,"2018-08-15","12:25:00","EST",{"$nulls":4},130,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734865744","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,130,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14438.CHEM/results/734865744/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-09-24T10:45:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14059.CHEM","Sample-Routine","Other",null,"2018-02-08","12:00:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61874",81564,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.6230583,-111.7158139,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734915947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14059.CHEM/results/734915947/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2018-09-24T10:51:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14057.CHEM","Sample-Routine","Other",null,"2018-05-24","10:45:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61925",81613,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},31.9654694,-110.2871444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734911912","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8,N1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14057.CHEM/results/734911912/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2018-09-24T10:51:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14072.CHEM","Sample-Routine","Other",null,"2018-02-02","03:30:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-52797",63335,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734875637","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: D2,E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14072.CHEM/results/734875637/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",{"$nulls":3},"2018-09-24T10:46:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB17533.CHEM","Sample-Routine","Other",null,"2019-02-14","12:03:00","EST",{"$nulls":4},103.32,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-781050550","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,103.32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB17533.CHEM/results/781050550/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2019-03-28T10:25:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29058.CHEM","Sample-Routine","Other","Groundwater","2019-12-10","11:12:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859908756","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29058.CHEM/results/859908756/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28844.CHEM","Sample-Routine","Other","Groundwater","2019-10-01","03:43:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856013999","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28844.CHEM/results/856013999/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2020-09-10T09:53:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18531.CHEM","Sample-Routine","Water","Groundwater","2019-01-10","09:45:00","EST",{"$nulls":4},320,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-788208661","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,320,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18531.CHEM/results/788208661/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2019-05-29T09:08:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29083.CHEM","Sample-Routine","Other","Groundwater","2019-12-12","11:27:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859910381","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29083.CHEM/results/859910381/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29063.CHEM","Sample-Routine","Other","Groundwater","2019-12-11","02:44:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909081","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29063.CHEM/results/859909081/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29988.CHEM","Sample-Routine","Water","Groundwater","2019-04-12","08:43:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62349",81845,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7210566,-112.0000018,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872413552","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29988.CHEM/results/872413552/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2021-01-19T10:34:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30395.CHEM","Sample-Routine","Water","Groundwater","2019-11-18","06:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","ARIZONA DEPT OF ENVIRONMENTAL QUALITY","AZDEQ_WPD-61908",81596,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3108433,-111.0353167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-875255291","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30395.CHEM/results/875255291/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2021-02-08T10:56:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28081.CHEM","Sample-Routine","Water","Groundwater","2019-12-03","10:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804068","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28081.CHEM/results/849804068/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2020-06-22T11:29:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25015.CHEM","Sample-Routine","Water","Groundwater","2019-11-19","09:11:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52799",63337,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2019433,-110.9690472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-827751386","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25015.CHEM/results/827751386/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-03-13T11:23:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29065.CHEM","Sample-Routine","Other","Groundwater","2019-12-10","02:39:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909211","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29065.CHEM/results/859909211/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29067.CHEM","Sample-Routine","Other","Groundwater","2019-12-10","10:45:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909341","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29067.CHEM/results/859909341/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26156.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","12:05:00","MST",{"$nulls":4},119,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-51311",61440,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4320528,-112.0987861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832560449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},119,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26156.CHEM/results/832560449/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-07T11:05:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28845.CHEM","Sample-Routine","Other","Groundwater","2019-10-02","02:20:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856014067","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28845.CHEM/results/856014067/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2020-09-10T09:53:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29977.CHEM","Sample-Routine","Water","Groundwater","2019-01-31","09:28:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62348",81844,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7210559,-112.0000017,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872412738","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29977.CHEM/results/872412738/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2021-01-19T10:33:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26166.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","03:32:00","MST",{"$nulls":4},225,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62400",81882,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4270989,-112.0871484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832561476","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},225,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26166.CHEM/results/832561476/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-07T11:05:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29764.CHEM","Sample-Routine","Water","Groundwater","2020-11-05","10:15:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52862",63334,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2014664,-110.9687608,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871461944","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29764.CHEM/results/871461944/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2020-12-28T09:36:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32893.CHEM","Sample-Routine","Water","Groundwater","2020-10-14","01:20:00","MST",{"$nulls":4},137,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56712",72041,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3582617,-111.8110453,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905983805","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,137,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32893.CHEM/results/905983805/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29269.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","10:27:00","MST",{"$nulls":4},42,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50199",62104,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4877681,-111.9961122,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860613171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,42,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29269.CHEM/results/860613171/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30370.CHEM","Sample-Routine","Water","Groundwater","2020-11-12","10:30:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58666",79062,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5088167,-112.0496333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765561","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30370.CHEM/results/874765561/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2021-02-04T10:52:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29299.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","12:31:00","MST",{"$nulls":4},156,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62051",81662,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4827923,-111.9998295,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616127","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,156,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29299.CHEM/results/860616127/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26382.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-03-13","12:00:00","MST",{"$nulls":4},185,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-58425",78221,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4330189,-112.0983989,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839245555","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},185,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26382.CHEM/results/839245555/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-22T09:29:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26379.CHEM","Sample-Routine","Water","Groundwater","2020-03-11","10:00:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62401",81883,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4289567,-112.0911729,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839248585","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26379.CHEM/results/839248585/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-22T09:30:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28091.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","11:40:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804808","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28091.CHEM/results/849804808/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2020-06-22T11:29:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32887.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","07:40:00","MST",{"$nulls":4},333,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905983367","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,333,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32887.CHEM/results/905983367/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26745.CHEM","Sample-Routine","Water","Groundwater","2020-04-07","07:15:00","MST",{"$nulls":4},129,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58623",78963,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3565861,-111.8082917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-844184027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,129,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26745.CHEM/results/844184027/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2020-04-27T15:05:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30386.CHEM","Sample-Routine","Water","Groundwater","2020-12-16","05:14:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62548",81983,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2126345,-112.7551879,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-875254505","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30386.CHEM/results/875254505/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-02-08T10:56:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29308.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","11:52:00","MST",{"$nulls":4},87.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58925",79644,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4867869,-111.9982147,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,87.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29308.CHEM/results/860616793/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25042.CHEM","Sample-Routine","Water","Groundwater","2020-01-21","12:38:00","MST",{"$nulls":4},13.83,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","WESTERN TECHNOLOGY INC.","AZDEQ_WPD-61725",81432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0346639,-110.7223667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-829101919","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,13.83,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25042.CHEM/results/829101919/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2020-03-18T11:28:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29936.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","12:35:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62548",81983,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2126345,-112.7551879,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872129395","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29936.CHEM/results/872129395/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-01-12T11:32:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29305.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","09:54:00","MST",{"$nulls":4},220,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616571","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,220,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29305.CHEM/results/860616571/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28326.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","10:40:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50272",60375,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5087536,-112.0739797,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123170","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28326.CHEM/results/850123170/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2020-07-06T11:16:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29282.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","12:24:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62050",81661,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4765057,-112.0172709,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860614503","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29282.CHEM/results/860614503/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32877.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","07:21:00","MST",{"$nulls":4},331,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-47634",57289,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271944,-110.8376042,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905982637","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,331,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32877.CHEM/results/905982637/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32896.CHEM","Sample-Routine","Water","Groundwater","2020-10-14","12:12:00","MST",{"$nulls":4},137,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56713",72042,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3622472,-111.8090983,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905984024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,137,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32896.CHEM/results/905984024/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29777.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","11:30:00","MST",{"$nulls":4},117,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54635",62158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.00218,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},117,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29777.CHEM/results/871506748/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2020-12-30T18:52:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29313.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","01:36:00","MST",{"$nulls":4},225,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62052",81663,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4730179,-112.0239066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860617163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,225,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29313.CHEM/results/860617163/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25648.CHEM","Sample-Routine","Water","Groundwater","2020-02-12","12:00:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52698",63128,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016983,-110.9688897,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-829618457","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25648.CHEM/results/829618457/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-03-25T08:43:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32900.CHEM","Sample-Routine","Water","Groundwater","2020-10-14","08:20:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58522",78621,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4462683,-112.35735,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905984316","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32900.CHEM/results/905984316/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29332.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","10:16:00","MST",{"$nulls":4},71,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50838",60962,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4793619,-112.01496,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919900748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,71,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29332.CHEM/results/919900748/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-12-01T09:39:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43750.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-10","12:00:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992951514","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43750.CHEM/results/992951514/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43723.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","01:54:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61627",81371,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49253,-112.00725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992949516","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43723.CHEM/results/992949516/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35354.CHEM","Sample-Routine","Water","Groundwater","2021-12-22","04:29:00","MST",{"$nulls":4},101,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63017",82381,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8793896,-111.735863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994635345","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,V1.",null,101,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35354.CHEM/results/994635345/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2023-12-04T10:15:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30476.CHEM","Sample-Routine","Water","Groundwater","2021-01-21","12:13:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62645",82052,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184395,-110.6843498,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-879852522","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30476.CHEM/results/879852522/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2021-03-05T16:20:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43500.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","10:14:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-966047266","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43500.CHEM/results/966047266/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-01-30T10:12:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33341.CHEM","Sample-Routine","Water","Groundwater","2021-09-01","10:06:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62874",82245,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2562309,-114.1468746,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916469217","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33341.CHEM/results/916469217/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:15:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36508.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-03","03:41:00","MST",{"$nulls":4},215.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62912",82282,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387948,-112.1870131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937426609","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},215.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36508.CHEM/results/937426609/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2022-05-03T12:38:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30469.CHEM","Sample-Routine","Water","Groundwater","2021-01-20","06:50:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62642",82049,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186834,-110.6842638,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-879851885","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30469.CHEM/results/879851885/resdetectqntlmts","Laboratory Reporting Level",5.98,"ug/L",{"$nulls":3},"2021-03-05T16:20:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33256.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","01:51:00","MST",{"$nulls":4},208,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62251",81754,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4716569,-112.0263153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916460363","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,208,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33256.CHEM/results/916460363/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33043.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","10:34:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62847",82218,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0268341,-110.7069226,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916456813","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33043.CHEM/results/916456813/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-10-19T11:11:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35007.CHEM","Sample-Routine","Water","Groundwater","2021-12-21","03:35:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52799",63337,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2019433,-110.9690472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994628978","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35007.CHEM/results/994628978/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44882.CHEM","Sample-Routine","Water","Groundwater","2021-06-03","08:29:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62483",81930,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4953,-112.00041,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974184567","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44882.CHEM/results/974184567/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-05T10:03:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38267.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","12:43:00","MST",{"$nulls":4},39.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63106",82432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2859565,-110.1178806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943317605","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},39.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38267.CHEM/results/943317605/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",{"$nulls":3},"2022-07-05T13:19:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35576.CHEM","Sample-Routine","Water","Groundwater","2021-09-21","08:50:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47010",56622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048881,-112.1491475,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933547117","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35576.CHEM/results/933547117/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-03-25T10:44:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43691.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","01:35:00","MST",{"$nulls":4},228,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61627",81371,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49253,-112.00725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992947148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},228,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43691.CHEM/results/992947148/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37344.CHEM","Sample-Routine","Water","Groundwater","2021-10-28","11:04:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943308120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37344.CHEM/results/943308120/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-07-05T13:15:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43758.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","03:08:00","MST",{"$nulls":4},120,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63287",82605,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.492633,-112.0111495,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992952106","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},120,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43758.CHEM/results/992952106/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:50","STORET"]
["AZDEQ_GW","AZDEQ_GW","AZDEQ_GW-AB47877.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","11:15:00","MST",{"$nulls":4},168,"ft",{"$nulls":5},9876,"2023_WQARF","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_GW-53299",64038,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4993,-112.1446278,"Unknown","AZDEQ_GW","Unknown",null,"Miscellaneous (Other)","STORET-988029504","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},168,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_GW","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_GW/activities/AZDEQ_GW-AB47877.CHEM/results/988029504/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-09-06T10:11:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33312.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","05:33:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62743",82131,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0191229,-110.6824885,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916500086","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33312.CHEM/results/916500086/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-10-21T10:57:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44883.CHEM","Sample-Routine","Water","Groundwater","2021-05-26","01:19:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974184646","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44883.CHEM/results/974184646/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-05T10:03:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35739.CHEM","Sample-Routine","Water","Groundwater","2021-12-02","08:39:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63069",82403,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483984,-112.149587,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994515857","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35739.CHEM/results/994515857/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-02T11:38:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38274.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","11:30:00","MST",{"$nulls":4},43,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63083",82409,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860822,-110.1179399,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943318123","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},43,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38274.CHEM/results/943318123/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2022-07-05T13:20:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33995.CHEM","Sample-Routine","Water","Groundwater","2021-09-30","10:31:00","MST",{"$nulls":4},73.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-51181",61309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4801809,-112.0133971,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919900928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,73.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33995.CHEM/results/919900928/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-12-01T09:40:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32936.CHEM","Sample-Routine","Water","Groundwater","2021-08-09","03:09:00","MST",{"$nulls":4},209,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62820",82198,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7652751,-112.4536329,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-914941618","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,209,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32936.CHEM/results/914941618/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-10-01T11:40:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33342.CHEM","Sample-Routine","Water","Groundwater","2021-09-01","07:36:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62673",82078,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2561063,-114.146959,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916469309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5,V1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33342.CHEM/results/916469309/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:15:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33076.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","08:38:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50237",60340,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3779486,-111.8246017,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916457033","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33076.CHEM/results/916457033/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:11:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43499.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","09:33:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-966047191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43499.CHEM/results/966047191/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-01-30T10:12:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32941.CHEM","Sample-Routine","Water","Groundwater","2021-08-09","03:42:00","MST",{"$nulls":4},210,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62826",82204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651708,-112.4536862,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-914941938","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,210,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32941.CHEM/results/914941938/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-10-01T11:40:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36501.CHEM","Sample-Routine","Water","Groundwater","2021-12-03","12:25:00","MST",{"$nulls":4},215,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62916",82286,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5388076,-112.1871246,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937426091","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},215,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36501.CHEM/results/937426091/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-05-03T12:37:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48312.CHEM","Sample-Routine","Water","Groundwater","2021-11-17","09:00:00","MST",{"$nulls":4},125,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63194",82513,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7362398,-112.0100517,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993004319","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},125,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48312.CHEM/results/993004319/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2023-11-09T09:47:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32920.CHEM","Sample-Routine","Water","Groundwater","2021-07-20","08:09:00","MST",{"$nulls":4},345,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-906967356","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,N1.",null,345,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32920.CHEM/results/906967356/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-09T21:59:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35005.CHEM","Sample-Routine","Water","Groundwater","2021-12-19","03:24:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52862",63334,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2014664,-110.9687608,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994628793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35005.CHEM/results/994628793/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35590.CHEM","Sample-Routine","Water","Groundwater","2021-09-23","10:40:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63056",82390,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484119,-112.1499339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933548167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35590.CHEM/results/933548167/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-03-25T10:45:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34976.CHEM","Sample-Routine","Water","Groundwater","2021-12-02","09:47:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62655",82062,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0183469,-110.6844878,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994507876","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34976.CHEM/results/994507876/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2023-12-02T11:38:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34207.CHEM","Sample-Routine","Water","Groundwater","2021-11-16","12:05:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52695",63125,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2026803,-110.9690714,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-925214930","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34207.CHEM/results/925214930/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-12-28T10:27:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34175.CHEM","Sample-Routine","Water","Groundwater","2021-11-30","09:41:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62875",82246,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560792,-114.1470676,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994247452","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34175.CHEM/results/994247452/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-30T10:14:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43433.CHEM","Sample-Routine","Water","Groundwater","2021-11-18","01:15:00","MST",{"$nulls":4},295,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62811",82190,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5032469,-112.1732619,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992939378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},295,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43433.CHEM/results/992939378/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33021.CHEM","Sample-Routine","Water","Groundwater","2021-08-20","03:29:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52797",63335,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916464169","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33021.CHEM/results/916464169/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",{"$nulls":3},"2021-10-19T11:13:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33202.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","06:54:00","MST",{"$nulls":4},148,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62005",81652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.365538,-111.8222295,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916461251","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,148,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33202.CHEM/results/916461251/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32913.CHEM","Sample-Routine","Water","Groundwater","2021-07-20","06:52:00","MST",{"$nulls":4},330,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62099",81698,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3595803,-110.8348695,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-906966873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,N1.",null,330,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32913.CHEM/results/906966873/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-09T21:59:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37395.CHEM","Sample-Routine","Water","Groundwater","2021-10-22","12:30:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62249",81752,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5038102,-112.0479517,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943311080","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37395.CHEM/results/943311080/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-07-05T13:16:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34988.CHEM","Sample-Routine","Water","Groundwater","2021-11-30","12:19:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62742",82130,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0197062,-110.68312,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994250696","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34988.CHEM/results/994250696/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-30T10:14:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37340.CHEM","Sample-Routine","Water","Groundwater","2021-10-27","02:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943307824","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37340.CHEM/results/943307824/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-07-05T13:15:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33253.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","01:07:00","MST",{"$nulls":4},245,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62052",81663,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4730179,-112.0239066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916460141","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,245,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33253.CHEM/results/916460141/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34061.CHEM","Sample-Routine","Water","Groundwater","2021-11-09","01:56:00","MST",{"$nulls":4},209,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62826",82204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651708,-112.4536862,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-921314941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,209,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34061.CHEM/results/921314941/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-12-06T09:11:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32921.CHEM","Sample-Routine","Water","Groundwater","2021-07-20","07:50:00","MST",{"$nulls":4},345,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62133",81708,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271694,-110.8374424,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-906967425","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,N1.",null,345,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32921.CHEM/results/906967425/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-09T21:59:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33216.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","10:20:00","MST",{"$nulls":4},142,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58622",78962,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3597333,-111.8042472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916462287","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,142,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33216.CHEM/results/916462287/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:13:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44914.CHEM","Sample-Routine","Water","Groundwater","2021-05-25","11:26:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54635",62158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.00218,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974187048","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44914.CHEM/results/974187048/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-05T10:07:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43736.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","03:44:00","MST",{"$nulls":4},118,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-40429",46747,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49439,-112.00447,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992950478","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},118,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43736.CHEM/results/992950478/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33210.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","09:21:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56714",72043,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3639236,-111.8073342,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916461843","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33210.CHEM/results/916461843/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38951.CHEM","Sample-Routine","Water","Groundwater","2022-04-01","09:40:00","MST",{"$nulls":4},97,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62940",82306,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834931,-110.7759672,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-950632947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},97,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38951.CHEM/results/950632947/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-08-30T11:00:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43071.CHEM","Sample-Routine","Water","Groundwater","2022-12-27","04:28:00","MST",{"$nulls":4},43,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62873",82244,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529041,-110.0338758,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994681324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,Q7.",null,43,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43071.CHEM/results/994681324/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:19:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42926.CHEM","Sample-Routine","Water","Groundwater","2022-06-16","10:56:00","MST",{"$nulls":4},500,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63495",82807,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4843917,-111.7324554,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992928137","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,500,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42926.CHEM/results/992928137/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40275.CHEM","Sample-Routine","Water","Groundwater","2022-09-23","03:54:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62546",81981,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2122863,-112.7554876,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956948745","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40275.CHEM/results/956948745/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-10-28T11:00:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43537.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","01:58:00","MST",{"$nulls":4},125,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63304",82622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4921451,-114.3471484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992941820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,125,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43537.CHEM/results/992941820/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37117.CHEM","Sample-Routine","Water","Groundwater","2022-05-20","02:20:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52816",63357,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016572,-110.9689964,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994653237","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37117.CHEM/results/994653237/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35752.CHEM","Sample-Routine","Water","Groundwater","2022-02-18","05:15:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52797",63335,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994637427","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35752.CHEM/results/994637427/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",{"$nulls":3},"2023-12-04T10:15:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39336.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","10:14:00","MST",{"$nulls":4},172,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62821",82199,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.765276,-112.4536326,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994662250","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,172,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39336.CHEM/results/994662250/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49851.CHEM","Sample-Routine","Water","Groundwater","2022-02-17","12:10:00","MST",{"$nulls":4},227,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63152",82471,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5192136,-112.0810416,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999764669","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,227,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49851.CHEM/results/999764669/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2024-01-19T08:41:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41694.CHEM","Sample-Routine","Water","Groundwater","2022-11-18","09:45:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62647",82054,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0199058,-110.6829579,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994680010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41694.CHEM/results/994680010/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:19:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41241.CHEM","Sample-Routine","Water","Groundwater","2022-06-03","07:55:00","MST",{"$nulls":4},38,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62992",82358,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3360028,-110.9413239,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994673755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},38,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41241.CHEM/results/994673755/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:18:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48151.CHEM","Sample-Routine","Water","Groundwater","2022-05-12","09:35:00","MST",{"$nulls":4},65,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63191",82510,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7237579,-112.00439,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361026","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},65,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48151.CHEM/results/997361026/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-12-29T09:53:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35266.CHEM","Sample-Routine","Water","Groundwater","2022-02-08","01:28:00","MST",{"$nulls":4},215.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62826",82204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651708,-112.4536862,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994632940","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,215.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35266.CHEM/results/994632940/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:14:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35758.CHEM","Sample-Routine","Water","Groundwater","2022-02-14","03:21:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52695",63125,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2026803,-110.9690714,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994637994","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35758.CHEM/results/994637994/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:15:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35267.CHEM","Sample-Routine","Water","Groundwater","2022-02-08","09:45:00","MST",{"$nulls":4},205,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62820",82198,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7652751,-112.4536329,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994633004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,205,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35267.CHEM/results/994633004/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:14:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36944.CHEM","Sample-Routine","Water","Groundwater","2022-05-09","09:57:00","MST",{"$nulls":4},205.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62820",82198,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7652751,-112.4536329,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994648250","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,205.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36944.CHEM/results/994648250/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:16:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39476.CHEM","Sample-Routine","Water","Groundwater","2022-09-06","04:38:00","MST",{"$nulls":4},36.8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62868",82239,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2528438,-110.0338152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663221","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,36.8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39476.CHEM/results/994663221/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40277.CHEM","Sample-Routine","Water","Groundwater","2022-09-22","03:00:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62547",81982,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.212638,-112.7553669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956948929","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40277.CHEM/results/956948929/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2022-10-28T11:00:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39588.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","11:00:00","MST",{"$nulls":4},42,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63095",82421,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860355,-110.1180487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667773","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},42,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39588.CHEM/results/953667773/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",{"$nulls":3},"2022-10-12T10:05:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36021.CHEM","Sample-Routine","Water","Groundwater","2022-03-11","10:46:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62840",82211,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0267533,-110.7072866,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994642426","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: R7.",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36021.CHEM/results/994642426/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37467.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","06:54:00","MST",{"$nulls":4},180,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62692",82097,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5083552,-112.0731066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},180,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37467.CHEM/results/992902357/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39197.CHEM","Sample-Routine","Water","Groundwater","2022-08-19","01:47:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62576",82010,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7238778,-111.9985028,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992909186","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39197.CHEM/results/992909186/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48812.CHEM","Sample-Routine","Water","Groundwater","2022-08-30","01:00:00","MST",{"$nulls":4},159,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62560",81995,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945731,-114.6214489,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993010199","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},159,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48812.CHEM/results/993010199/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",{"$nulls":3},"2023-11-09T09:48:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39490.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","09:02:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50239",60342,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3780447,-111.8244892,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992912071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39490.CHEM/results/992912071/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:37:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40413.CHEM","Sample-Routine","Water","Groundwater","2022-01-17","11:15:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-62424",81900,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0674205,-112.1518977,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999446746","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40413.CHEM/results/999446746/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-16T10:10:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41526.CHEM","Sample-Routine","Water","Groundwater","2022-11-23","01:34:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52698",63128,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016983,-110.9688897,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994676743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41526.CHEM/results/994676743/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:19:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37140.CHEM","Sample-Routine","Water","Groundwater","2022-05-24","05:17:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62551",81986,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9010599,-110.1597276,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992894596","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37140.CHEM/results/992894596/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:36:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41737.CHEM","Sample-Routine","Water","Groundwater","2022-03-28","07:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-5035",10129,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.488105,-111.7301342,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992926257","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41737.CHEM/results/992926257/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41629.CHEM","Sample-Routine","Water","Groundwater","2022-11-30","02:35:00","MST",{"$nulls":4},70.74,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962654831","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},70.74,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41629.CHEM/results/962654831/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",{"$nulls":3},"2023-01-06T10:30:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48470.CHEM","Sample-Routine","Water","Groundwater","2022-09-06","09:45:00","MST",{"$nulls":4},164,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61854",81546,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4995459,-112.1452744,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993002017","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},164,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48470.CHEM/results/993002017/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43532.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-08-10","12:00:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62815",82194,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.488799,-114.3461386,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992941450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43532.CHEM/results/992941450/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37470.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","05:40:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49517",59450,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089358,-112.0742047,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37470.CHEM/results/992902579/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41631.CHEM","Sample-Routine","Water","Groundwater","2022-11-30","03:24:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62940",82306,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834931,-110.7759672,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962655010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41631.CHEM/results/962655010/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-01-06T10:31:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39299.CHEM","Sample-Routine","Water","Groundwater","2022-08-24","05:39:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62638",82045,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0189569,-110.6844168,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994660760","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39299.CHEM/results/994660760/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43890.CHEM","Sample-Routine","Other","Groundwater","2022-11-28","12:24:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954351","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43890.CHEM/results/992954351/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:42:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47535.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","07:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62563",81998,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4994189,-112.1458556,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992988600","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47535.CHEM/results/992988600/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43875.CHEM","Sample-Routine","Water","Groundwater","2022-11-17","10:21:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992952846","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43875.CHEM/results/992952846/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38524.CHEM","Sample-Routine","Water","Groundwater","2022-05-18","03:23:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49182",59108,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2208333,-114.5638889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994658240","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38524.CHEM/results/994658240/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41256.CHEM","Sample-Routine","Water","Groundwater","2022-06-01","05:55:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994674890","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41256.CHEM/results/994674890/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",{"$nulls":3},"2023-12-04T10:19:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40575.CHEM","Sample-Routine","Water","Groundwater","2022-01-25","11:00:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63517",82829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2122569,-110.9686374,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999758140","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40575.CHEM/results/999758140/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-19T08:41:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39697.CHEM","Sample-Routine","Other","Groundwater","2022-04-20","01:26:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-954060224","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39697.CHEM/results/954060224/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2022-10-14T11:13:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39219.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","01:45:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62567",82001,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7373778,-112.0074722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992910814","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39219.CHEM/results/992910814/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35000.CHEM","Sample-Routine","Water","Groundwater","2022-01-12","04:05:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-61874",81564,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.6230583,-111.7158139,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994628343","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: M1,M2,R2.",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35000.CHEM/results/994628343/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49116.CHEM","Sample-Routine","Water","Groundwater","2022-09-20","05:22:00","MST",{"$nulls":4},327.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62775",82154,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4867908,-112.100564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993015248","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},327.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49116.CHEM/results/993015248/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35497.CHEM","Sample-Routine","Water","Groundwater","2022-03-01","10:28:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62543",81978,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934,-111.9863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992884706","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35497.CHEM/results/992884706/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:35:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36044.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-03","12:00:00","MST",{"$nulls":4},16,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47011",56623,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482379,-112.1500859,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994643479","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},16,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36044.CHEM/results/994643479/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43039.CHEM","Sample-Routine","Water","Groundwater","2022-11-05","01:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-53890",64948,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2288028,-110.97026,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992932718","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43039.CHEM/results/992932718/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39303.CHEM","Sample-Routine","Water","Groundwater","2022-08-27","12:12:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62741",82129,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0193875,-110.6822587,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994661128","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39303.CHEM/results/994661128/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37464.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-04-06","12:00:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49518",59451,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.508745,-112.0739306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37464.CHEM/results/992902135/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43545.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","07:09:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63297",82615,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4859476,-114.3529682,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992942412","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,60,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43545.CHEM/results/992942412/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41505.CHEM","Sample-Routine","Water","Groundwater","2022-11-22","02:25:00","MST",{"$nulls":4},38.76,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63095",82421,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860355,-110.1180487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969238725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},38.76,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41505.CHEM/results/969238725/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",{"$nulls":3},"2023-03-03T09:05:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39233.CHEM","Sample-Routine","Water","Groundwater","2022-08-27","04:40:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52690",63120,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016586,-110.9696389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994658711","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39233.CHEM/results/994658711/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40724.CHEM","Sample-Routine","Water","Groundwater","2022-03-22","02:35:00","MST",{"$nulls":4},345,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59141",80388,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4993939,-111.7181111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992920041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,345,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40724.CHEM/results/992920041/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:38:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41169.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","04:40:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63057",82391,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483738,-112.1498945,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994670087","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41169.CHEM/results/994670087/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39222.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","03:05:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62599",82033,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7368583,-112.0076694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992911036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39222.CHEM/results/992911036/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43229.CHEM","Sample-Routine","Water","Groundwater","2022-10-14","02:30:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54036",65204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5087114,-112.0465083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999650799","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43229.CHEM/results/999650799/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-18T09:30:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39181.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","09:55:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62585",82019,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7239944,-112.0012278,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908002","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39181.CHEM/results/992908002/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43796.CHEM","Sample-Routine","Water","Groundwater","2022-12-07","09:52:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62977",82343,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.335875,-110.9417802,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994685898","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43796.CHEM/results/994685898/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:20:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39188.CHEM","Sample-Routine","Water","Groundwater","2022-08-19","09:20:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62682",82087,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7311444,-112.0063889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39188.CHEM/results/992908520/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47539.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","10:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55525",68579,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5005161,-112.1482836,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992988896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47539.CHEM/results/992988896/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43346.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-04","12:00:00","MST",{"$nulls":4},208,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63272",82590,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5167132,-112.176642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992938268","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},208,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43346.CHEM/results/992938268/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41187.CHEM","Sample-Routine","Water","Groundwater","2022-09-12","12:13:00","MST",{"$nulls":4},100.49,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63018",82382,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8788259,-111.7362534,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994671435","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,100.49,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41187.CHEM/results/994671435/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40676.CHEM","Sample-Routine","Water","Groundwater","2022-05-11","09:13:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63536",82848,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152112,-110.1515416,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994668952","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40676.CHEM/results/994668952/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:18:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43799.CHEM","Sample-Routine","Water","Groundwater","2022-12-07","11:57:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62983",82349,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357611,-110.9416976,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994686122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43799.CHEM/results/994686122/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:20:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36526.CHEM","Sample-Routine","Water","Groundwater","2022-03-09","12:47:00","MST",{"$nulls":4},101,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63021",82385,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8801621,-111.7359074,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994645679","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,101,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36526.CHEM/results/994645679/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:16:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47502.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","10:00:00","MST",{"$nulls":4},230,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48036",57704,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2285256,-111.3335314,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},230,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47502.CHEM/results/992986163/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",{"$nulls":3},"2023-11-09T09:45:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47768.CHEM","Sample-Routine","Water","Groundwater","2022-04-11","02:00:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62521",81958,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.525761,-112.081087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992990083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47768.CHEM/results/992990083/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37039.CHEM","Sample-Routine","Water","Groundwater","2022-05-10","04:10:00","MST",{"$nulls":4},23,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47008",56620,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0476764,-112.1489107,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,23,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37039.CHEM/results/994650029/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40416.CHEM","Sample-Routine","Water","Groundwater","2022-01-18","12:00:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-62429",81905,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0683157,-112.1514167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999647398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40416.CHEM/results/999647398/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-18T09:29:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40667.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","10:24:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63529",82841,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152602,-110.1537538,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994668278","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40667.CHEM/results/994668278/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:18:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43508.CHEM","Sample-Routine","Water","Groundwater","2022-08-09","04:56:00","MST",{"$nulls":4},155,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62690",82095,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4907601,-114.3477968,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992939674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},155,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43508.CHEM/results/992939674/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47542.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","08:20:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-53300",64039,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4976944,-112.1456028,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992989119","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47542.CHEM/results/992989119/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41168.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","01:17:00","MST",{"$nulls":4},24,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63066",82400,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481667,-112.1489083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994670013","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,24,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41168.CHEM/results/994670013/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43343.CHEM","Sample-Routine","Water","Groundwater","2022-03-04","11:20:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63274",82592,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4991517,-112.16619180000001,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992938046","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43343.CHEM/results/992938046/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38582.CHEM","Sample-Routine","Water","Groundwater","2022-06-07","02:48:00","MST",{"$nulls":4},10.9,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62855",82226,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2545888,-110.0306365,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994656309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},10.9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38582.CHEM/results/994656309/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48156.CHEM","Sample-Routine","Water","Groundwater","2022-05-11","02:20:00","MST",{"$nulls":4},75,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63195",82514,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.736204,-112.010142,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994876152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48156.CHEM/results/994876152/resdetectqntlmts","Laboratory Reporting Level",2.99000000953674,"ug/L",{"$nulls":3},"2023-12-06T15:47:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35680.CHEM","Sample-Routine","Water","Groundwater","2022-02-24","04:51:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62779",82158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.212335,-112.7553257,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994635986","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35680.CHEM/results/994635986/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:15:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37446.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","01:20:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54184",61809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5104497,-112.0743658,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37446.CHEM/results/992900803/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43083.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","10:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62099",81698,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3595803,-110.8348695,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992933753","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43083.CHEM/results/992933753/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:39:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41689.CHEM","Sample-Routine","Water","Groundwater","2022-11-16","03:45:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62644",82051,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0185409,-110.6841669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679547","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41689.CHEM/results/994679547/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2023-12-04T10:19:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41509.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-11-22","01:15:00","MST",{"$nulls":4},32.09,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63092",82418,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2861373,-110.1179947,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969239052","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},32.09,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41509.CHEM/results/969239052/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-03-03T09:05:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35217.CHEM","Sample-Routine","Water","Groundwater","2022-01-19","06:13:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62377",81859,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2205364,-114.5641411,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994631838","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35217.CHEM/results/994631838/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36513.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","10:16:00","MST",{"$nulls":4},25.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63001",82366,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.5067521,-109.3643126,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937787377","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},25.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36513.CHEM/results/937787377/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-05-05T10:33:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43079.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","11:47:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992933457","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43079.CHEM/results/992933457/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:39:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43510.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","03:31:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63301",82619,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.492867,-114.3461749,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992939822","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43510.CHEM/results/992939822/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38474.CHEM","Sample-Routine","Water","Groundwater","2022-06-20","10:32:00","MST",{"$nulls":4},177.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62825",82203,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7648134,-112.4536487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994655252","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,177.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38474.CHEM/results/994655252/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:17:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43180.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-11-10","01:32:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63065",82399,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481968,-112.1490371,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994682759","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43180.CHEM/results/994682759/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:19:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43133.CHEM","Sample-Routine","Water","Groundwater","2022-12-16","11:15:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63536",82848,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152112,-110.1515416,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994687914","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43133.CHEM/results/994687914/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2023-12-04T10:20:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35856.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","12:38:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62993",82359,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357048,-110.9417694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994641295","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35856.CHEM/results/994641295/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2023-12-04T10:16:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45185.CHEM","Sample-Routine","Water","Groundwater","2022-10-17","05:10:00","MST",{"$nulls":4},120,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63286",82604,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4925483,-112.0072941,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992969367","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},120,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45185.CHEM/results/992969367/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:43:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39191.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","07:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62574",82008,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7279944,-112.0014028,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908742","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39191.CHEM/results/992908742/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37111.CHEM","Sample-Routine","Water","Groundwater","2022-05-19","02:32:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52690",63120,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016586,-110.9696389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994652684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37111.CHEM/results/994652684/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39572.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","10:35:00","MST",{"$nulls":4},50,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63127",82447,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7388939,-112.0078414,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953580071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},50,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39572.CHEM/results/953580071/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-10-07T10:34:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48453.CHEM","Sample-Routine","Water","Groundwater","2022-02-22","11:05:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62161",81716,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5249138,-112.0816383,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993002977","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48453.CHEM/results/993002977/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:47:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43542.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","02:15:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63304",82622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4921451,-114.3471484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992942190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43542.CHEM/results/992942190/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47976.CHEM","Sample-Routine","Water","Groundwater","2022-10-03","11:50:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-56983",72800,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5244731,-112.0829683,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992991387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47976.CHEM/results/992991387/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49843.CHEM","Sample-Routine","Water","Groundwater","2022-02-18","12:45:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62518",81955,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5257506,-112.0816368,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993026857","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49843.CHEM/results/993026857/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2023-11-09T09:49:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48457.CHEM","Quality Control Sample-Equipment Blank","Water","Groundwater","2022-02-22","09:15:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-53578",64410,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993003569","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48457.CHEM/results/993003569/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:47:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42954.CHEM","Sample-Routine","Water","Groundwater","2022-09-03","09:30:00","MST",{"$nulls":4},73,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59142",80389,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4988708,-111.7143906,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992930705","Not Detected",null,"1,3-Butadiene","Total",null,null,"J","Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES | QA FLAGS: J3.",null,73,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42954.CHEM/results/992930705/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2023-11-09T09:39:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35219.CHEM","Sample-Routine","Water","Groundwater","2022-01-21","04:10:00","MST",{"$nulls":4},28,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49223",59153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2213989,-114.5633969,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994632028","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,28,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35219.CHEM/results/994632028/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38744.CHEM","Sample-Routine","Water","Groundwater","2022-07-20","10:35:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62100",81699,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2262032,-110.8349466,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992906299","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38744.CHEM/results/992906299/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:37:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39582.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","08:40:00","MST",{"$nulls":4},26,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63089",82415,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2861544,-110.1178365,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},26,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39582.CHEM/results/953667329/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-10-12T10:05:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47985.CHEM","Sample-Routine","Water","Groundwater","2022-10-04","11:00:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-53578",64410,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992992059","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47985.CHEM/results/992992059/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47554.CHEM","Sample-Routine","Water","Groundwater","2022-04-29","06:50:00","MST",{"$nulls":4},167,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59250",81051,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4989258,-112.1439489,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992987785","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},167,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47554.CHEM/results/992987785/resdetectqntlmts","Laboratory Reporting Level",1.49000000953674,"ug/L",{"$nulls":3},"2023-11-09T09:45:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41715.CHEM","Sample-Routine","Water","Groundwater","2022-03-23","02:39:00","MST",{"$nulls":4},312,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47795",57463,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4750856,-111.7297614,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992924524","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,312,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41715.CHEM/results/992924524/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37040.CHEM","Sample-Routine","Water","Groundwater","2022-05-12","10:49:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63058",82392,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482178,-112.1488252,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650104","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37040.CHEM/results/994650104/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45342.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","08:25:00","MST",{"$nulls":4},50.6,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63097",82423,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2863196,-110.1181009,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974804387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},50.6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45342.CHEM/results/974804387/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-23T13:51:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47276.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","12:35:00","MST",{"$nulls":4},175,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62266",81767,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6944968,-114.6203508,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999215537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},175,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47276.CHEM/results/999215537/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-09T09:21:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47281.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","11:30:00","MST",{"$nulls":4},153,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62557",81992,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6951457,-114.6203806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999215909","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},153,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47281.CHEM/results/999215909/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-09T09:21:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47271.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","02:45:00","MST",{"$nulls":4},147,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61902",81590,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6935194,-114.6203461,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999215164","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},147,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47271.CHEM/results/999215164/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2024-01-09T09:20:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45171.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","01:38:00","MST",{"$nulls":4},36.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62868",82239,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2528438,-110.0338152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974992816","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,36.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45171.CHEM/results/974992816/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-25T10:52:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45493.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","02:21:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994694627","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1,.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45493.CHEM/results/994694627/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",{"$nulls":3},"2023-12-04T10:20:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48174.CHEM","Sample-Routine","Water","Groundwater","2023-01-30","01:40:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62060",81670,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6933939,-114.6214188,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992995337","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48174.CHEM/results/992995337/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2023-11-09T09:46:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48977.CHEM","Sample-Routine","Water","Groundwater","2023-01-17","02:18:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62776",82155,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.485781,-112.1016998,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993014730","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48977.CHEM/results/993014730/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49012.CHEM","Sample-Routine","Water","Groundwater","2023-03-30","12:23:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993019170","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49012.CHEM/results/993019170/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48192.CHEM","Sample-Routine","Water","Groundwater","2023-01-30","01:05:00","MST",{"$nulls":4},142,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55380",68281,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6932833,-114.6211361,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992996686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},142,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48192.CHEM/results/992996686/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44377.CHEM","Sample-Routine","Other","Groundwater","2023-02-10","02:54:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992962397","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44377.CHEM/results/992962397/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:43:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49041.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","02:30:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62234",81738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4949968,-112.0012566,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993021316","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49041.CHEM/results/993021316/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49019.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","10:35:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62235",81739,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947199,-112.0021762,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993019688","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49019.CHEM/results/993019688/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46323.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","10:40:00","MST",{"$nulls":4},164,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62562",81997,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4990217,-112.1466122,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992978667","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},164,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46323.CHEM/results/992978667/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:45:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48071.CHEM","Sample-Routine","Water","Groundwater","2023-01-25","03:45:00","MST",{"$nulls":4},160,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62554",81989,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945952,-114.6203669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992994588","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},160,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48071.CHEM/results/992994588/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49447.CHEM","Sample-Routine","Water","Groundwater","2023-03-06","01:00:00","MST",{"$nulls":4},230,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63154",82473,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5192115,-112.0806546,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993024280","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},230,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49447.CHEM/results/993024280/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50503.CHEM","Sample-Routine","Water","Groundwater","2023-06-02","09:28:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63071",82405,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0494496,-112.1508268,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706569","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,45,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50503.CHEM/results/994706569/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45534.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:49:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62860",82231,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.255927,-110.0234277,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45534.CHEM/results/975083729/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-30T10:53:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50512.CHEM","Sample-Routine","Water","Groundwater","2023-05-31","03:45:00","MST",{"$nulls":4},12,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47012",56624,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0477975,-112.1493457,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994707244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,12,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50512.CHEM/results/994707244/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46004.CHEM","Sample-Routine","Other","Groundwater","2023-05-04","03:32:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992976365","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46004.CHEM/results/992976365/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:44:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46003.CHEM","Sample-Routine","Other","Groundwater","2023-05-04","02:43:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992976297","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46003.CHEM/results/992976297/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:44:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46354.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","09:48:00","MST",{"$nulls":4},93,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62952",82318,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3836634,-110.776152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,93,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46354.CHEM/results/983662780/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49088.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","05:27:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62977",82343,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.335875,-110.9417802,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49088.CHEM/results/994705004/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49096.CHEM","Sample-Routine","Water","Groundwater","2023-06-08","08:34:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62988",82354,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.33581,-110.9417227,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705598","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49096.CHEM/results/994705598/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49097.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-07","04:26:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62989",82355,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359302,-110.9417269,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705672","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49097.CHEM/results/994705672/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50499.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","09:55:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63055",82389,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0487386,-112.1489839,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706269","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50499.CHEM/results/994706269/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46358.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","02:34:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62951",82317,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833447,-110.7755438,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983663076","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46358.CHEM/results/983663076/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46594.CHEM","Sample-Routine","Other","Groundwater","2023-05-10","10:56:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992983524","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46594.CHEM/results/992983524/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:45:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46344.CHEM","Sample-Routine","Water","Groundwater","2023-04-27","11:10:00","MST",{"$nulls":4},84,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: M1,R5,.",null,84,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46344.CHEM/results/983662034/resdetectqntlmts","Laboratory Reporting Level",5.98,"ug/L",{"$nulls":3},"2023-07-26T11:00:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46347.CHEM","Sample-Routine","Water","Groundwater","2023-04-26","12:38:00","MST",{"$nulls":4},74,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62938",82304,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833563,-110.7760749,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662257","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},74,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46347.CHEM/results/983662257/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48571.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","01:45:00","MST",{"$nulls":4},159,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-15970",24732,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6941992,-114.6281436,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993001343","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,159,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48571.CHEM/results/993001343/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49158.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","02:17:00","MST",{"$nulls":4},65,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016358","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},65,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49158.CHEM/results/993016358/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49161.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","12:47:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016580","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49161.CHEM/results/993016580/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46577.CHEM","Sample-Routine","Other","Groundwater","2023-05-11","04:45:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992982368","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46577.CHEM/results/992982368/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:45:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46222.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:20:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-54199",65608,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5280103,-112.0834631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992985027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46222.CHEM/results/992985027/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:45:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49085.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","10:35:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62978",82344,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358918,-110.9416598,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49085.CHEM/results/994704780/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45529.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:14:00","MST",{"$nulls":4},30.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62862",82233,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.255957,-110.0239318,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083461","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,30.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45529.CHEM/results/975083461/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-30T10:53:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49086.CHEM","Sample-Routine","Water","Groundwater","2023-06-08","11:50:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62979",82345,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357929,-110.9418056,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704854","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49086.CHEM/results/994704854/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48987.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","12:37:00","MST",{"$nulls":4},305,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62775",82154,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4867908,-112.100564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013990","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},305,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48987.CHEM/results/993013990/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50498.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","11:01:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47007",56619,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484,-112.148911,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706195","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50498.CHEM/results/994706195/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46345.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","12:56:00","MST",{"$nulls":4},96,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62945",82311,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.383618,-110.7758978,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},96,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46345.CHEM/results/983662109/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50501.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","03:34:00","MST",{"$nulls":4},6,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63056",82390,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484119,-112.1499339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706421","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50501.CHEM/results/994706421/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48546.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","10:55:00","MST",{"$nulls":4},165,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61907",81595,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6943898,-114.6224328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999760256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,165,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48546.CHEM/results/999760256/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-19T08:41:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50510.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","08:45:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47010",56622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048881,-112.1491475,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994707096","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50510.CHEM/results/994707096/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50506.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-02","11:37:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63061",82395,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483203,-112.1490083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706798","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,H1,.",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50506.CHEM/results/994706798/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46309.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","10:55:00","MST",{"$nulls":4},195,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55494",68499,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945844,-114.6232625,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992979185","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},195,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46309.CHEM/results/992979185/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:45:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46310.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","10:05:00","MST",{"$nulls":4},136,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62057",81667,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6938676,-114.6203393,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999651493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,136,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46310.CHEM/results/999651493/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2024-01-18T09:30:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49098.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-07","09:35:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62983",82349,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357611,-110.9416976,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705747","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49098.CHEM/results/994705747/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48983.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","11:04:00","MST",{"$nulls":4},134,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62774",82153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4868778,-112.1006288,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013694","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},134,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48983.CHEM/results/993013694/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49087.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","03:25:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49087.CHEM/results/994704928/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",{"$nulls":3},"2023-12-04T10:21:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46352.CHEM","Sample-Routine","Water","Groundwater","2023-04-26","10:48:00","MST",{"$nulls":4},103,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62941",82307,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3840379,-110.7762873,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},103,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46352.CHEM/results/983662632/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49082.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","02:56:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62985",82351,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359064,-110.9418538,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704551","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49082.CHEM/results/994704551/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48988.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","11:25:00","MST",{"$nulls":4},141,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62774",82153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4868778,-112.1006288,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993014064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},141,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48988.CHEM/results/993014064/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49092.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","04:15:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62984",82350,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358115,-110.9418872,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705300","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49092.CHEM/results/994705300/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48552.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","10:20:00","MST",{"$nulls":4},147,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61904",81592,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6940346,-114.6214261,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992999924","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},147,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48552.CHEM/results/992999924/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46604.CHEM","Sample-Routine","Other","Groundwater","2023-05-11","02:25:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992984204","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46604.CHEM/results/992984204/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:45:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48982.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-04-14","12:00:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62776",82155,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.485781,-112.1016998,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013620","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48982.CHEM/results/993013620/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48558.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","09:50:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62060",81670,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6933939,-114.6214188,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993000372","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48558.CHEM/results/993000372/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49167.CHEM","Sample-Routine","Water","Groundwater","2023-04-05","12:05:00","MST",{"$nulls":4},155,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993017024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},155,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49167.CHEM/results/993017024/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45531.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","02:34:00","MST",{"$nulls":4},28,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62859",82230,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2558122,-110.0239078,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083571","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,28,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45531.CHEM/results/975083571/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-30T10:53:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50985.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","12:41:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035265","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50985.CHEM/results/993035265/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51525.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","11:17:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52476",62766,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2259808,-110.9666858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038566","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51525.CHEM/results/993038566/resdetectqntlmts","Laboratory Reporting Level",0.0443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50984.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","09:31:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035197","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50984.CHEM/results/993035197/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51002.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:55:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036421","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51002.CHEM/results/993036421/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50996.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","12:05:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036013","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50996.CHEM/results/993036013/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50980.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","08:33:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034925","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50980.CHEM/results/993034925/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50893.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","10:36:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63479",82795,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9009139,-110.1588167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034449","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50893.CHEM/results/993034449/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50992.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","04:09:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035741","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50992.CHEM/results/993035741/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51533.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","01:10:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52475",62765,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258156,-110.9669394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993039110","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51533.CHEM/results/993039110/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51531.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","09:28:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63545",82856,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2259876,-110.9667495,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038974","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},45,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51531.CHEM/results/993038974/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50993.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","10:42:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62324",81825,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035809","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50993.CHEM/results/993035809/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50888.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","02:59:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034109","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50888.CHEM/results/993034109/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50988.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","12:43:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62338",81835,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035469","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50988.CHEM/results/993035469/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50983.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:01:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62333",81830,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035129","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50983.CHEM/results/993035129/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50987.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","10:51:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62322",81823,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035401","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50987.CHEM/results/993035401/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50986.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:44:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035333","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50986.CHEM/results/993035333/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50978.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","11:45:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034789","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50978.CHEM/results/993034789/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50974.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","03:33:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62314",81815,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034517","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50974.CHEM/results/993034517/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50982.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:57:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62340",81837,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035061","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50982.CHEM/results/993035061/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50995.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:57:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035945","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50995.CHEM/results/993035945/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51004.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","04:25:00","MST",{"$nulls":4},13.7,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62317",81818,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036557","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},13.7,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51004.CHEM/results/993036557/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50889.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","01:43:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63480",82796,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9007889,-110.1590667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034177","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50889.CHEM/results/993034177/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51529.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","12:21:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63546",82857,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258496,-110.9666718,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038838","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51529.CHEM/results/993038838/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51001.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","10:46:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036353","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51001.CHEM/results/993036353/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51527.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","03:35:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52474",62764,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258108,-110.9664744,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038702","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51527.CHEM/results/993038702/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50981.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","02:33:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034993","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50981.CHEM/results/993034993/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50998.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:14:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036149","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50998.CHEM/results/993036149/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50994.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","02:13:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035877","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50994.CHEM/results/993035877/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50976.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","12:10:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62337",81834,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034653","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50976.CHEM/results/993034653/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50891.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","02:38:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034313","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50891.CHEM/results/993034313/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51528.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:38:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63547",82858,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2260778,-110.9664476,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038770","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51528.CHEM/results/993038770/resdetectqntlmts","Laboratory Reporting Level",0.0443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51530.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:57:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63544",82855,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258612,-110.9668172,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038906","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51530.CHEM/results/993038906/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50989.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:42:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035537","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50989.CHEM/results/993035537/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50890.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","04:23:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034245","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50890.CHEM/results/993034245/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50991.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:32:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035673","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50991.CHEM/results/993035673/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51005.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","12:20:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036625","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51005.CHEM/results/993036625/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51526.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","01:24:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52473",62763,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2262686,-110.9664731,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038634","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51526.CHEM/results/993038634/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50997.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","10:13:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62311",81812,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232588,-110.972266,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036081","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50997.CHEM/results/993036081/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51532.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:18:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63543",82854,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2260615,-110.9666247,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993039042","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51532.CHEM/results/993039042/resdetectqntlmts","Laboratory Reporting Level",0.443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50979.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:03:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034857","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50979.CHEM/results/993034857/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50999.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","02:50:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036217","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50999.CHEM/results/993036217/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51003.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","11:24:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036489","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51003.CHEM/results/993036489/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50977.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","02:01:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62342",81839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034721","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50977.CHEM/results/993034721/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50975.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","03:49:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62315",81816,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034585","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50975.CHEM/results/993034585/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50892.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","03:35:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63478",82794,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9005639,-110.1590444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034381","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50892.CHEM/results/993034381/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50990.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","12:22:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62318",81819,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035605","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50990.CHEM/results/993035605/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51000.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:17:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036285","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51000.CHEM/results/993036285/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52416.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:03:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361574","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52416.CHEM/results/997361574/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52440.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","10:56:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363206","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52440.CHEM/results/997363206/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52430.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:10:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362526","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52430.CHEM/results/997362526/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52347.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","03:48:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323972","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52347.CHEM/results/997323972/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52415.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","01:36:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361506","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52415.CHEM/results/997361506/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52417.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:09:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62333",81830,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361642","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52417.CHEM/results/997361642/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52343.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","05:25:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63479",82795,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9009139,-110.1588167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323700","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52343.CHEM/results/997323700/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52345.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","03:14:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323836","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52345.CHEM/results/997323836/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52427.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:38:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62338",81835,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362322","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52427.CHEM/results/997362322/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52439.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:12:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363138","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52439.CHEM/results/997363138/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52432.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:36:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62318",81819,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362662","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52432.CHEM/results/997362662/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52433.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:24:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362730","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52433.CHEM/results/997362730/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52436.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:44:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62342",81839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362934","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52436.CHEM/results/997362934/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52344.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","04:51:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323768","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52344.CHEM/results/997323768/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52420.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:59:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361846","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52420.CHEM/results/997361846/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52434.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:46:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362798","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52434.CHEM/results/997362798/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52437.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:28:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62337",81834,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363002","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52437.CHEM/results/997363002/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52414.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:16:00","MST",{"$nulls":4},13.7,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62317",81818,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361438","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},13.7,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52414.CHEM/results/997361438/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52418.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:40:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62315",81816,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361710","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52418.CHEM/results/997361710/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52422.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:52:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361982","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52422.CHEM/results/997361982/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52426.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:54:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362254","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52426.CHEM/results/997362254/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52441.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:23:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62314",81815,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363274","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52441.CHEM/results/997363274/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52348.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","02:48:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63480",82796,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9007889,-110.1590667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997324040","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52348.CHEM/results/997324040/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52429.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","10:49:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362458","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52429.CHEM/results/997362458/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52435.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","11:30:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62311",81812,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232588,-110.972266,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362866","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52435.CHEM/results/997362866/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52428.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","01:12:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362390","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52428.CHEM/results/997362390/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52425.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","10:30:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362186","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52425.CHEM/results/997362186/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52411.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","11:13:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361234","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52411.CHEM/results/997361234/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52412.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:03:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361302","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52412.CHEM/results/997361302/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52438.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:56:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62322",81823,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363070","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52438.CHEM/results/997363070/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52346.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","04:22:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63478",82794,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9005639,-110.1590444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323904","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52346.CHEM/results/997323904/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52442.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:31:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62340",81837,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363342","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52442.CHEM/results/997363342/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52424.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:01:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362118","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52424.CHEM/results/997362118/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52419.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:46:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361778","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52419.CHEM/results/997361778/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52413.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","10:50:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361370","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52413.CHEM/results/997361370/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52431.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","02:02:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362594","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52431.CHEM/results/997362594/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52421.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:08:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361914","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52421.CHEM/results/997361914/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52423.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","12:40:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62324",81825,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362050","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52423.CHEM/results/997362050/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:48","STORET"]
[]
[{"$nulls":77},"mean",{"$f":"AVERAGE(CA2:CA3704)","v":0.03999999999999991},"ug/l"]
[{"$nulls":77},"median",{"$f":"MEDIAN(CA2:CA3704)","v":0.04},"ug/l"]

{"sheet":"Groundwater","index":5,"n_rows":10210,"n_cols":83,"rows_kept":1125,"cut":true,"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
["OrganizationIdentifier","OrganizationFormalName","ActivityIdentifier","ActivityTypeCode","ActivityMediaName","ActivityMediaSubdivisionName","ActivityStartDate","ActivityStartTime/Time","ActivityStartTime/TimeZoneCode","ActivityEndDate","ActivityEndTime/Time","ActivityEndTime/TimeZoneCode","ActivityRelativeDepthName","ActivityDepthHeightMeasure/MeasureValue","ActivityDepthHeightMeasure/MeasureUnitCode","ActivityDepthAltitudeReferencePointText","ActivityTopDepthHeightMeasure/MeasureValue","ActivityTopDepthHeightMeasure/MeasureUnitCode","ActivityBottomDepthHeightMeasure/MeasureValue","ActivityBottomDepthHeightMeasure/MeasureUnitCode","ProjectIdentifier","ProjectName","ActivityConductingOrganizationText","MonitoringLocationIdentifier","MonitoringLocationName","ActivityCommentText","SampleAquifer","HydrologicCondition","HydrologicEvent","ActivityLocation/LatitudeMeasure","ActivityLocation/LongitudeMeasure","SampleCollectionMethod/MethodIdentifier","SampleCollectionMethod/MethodIdentifierContext","SampleCollectionMethod/MethodName","SampleCollectionMethod/MethodDescriptionText","SampleCollectionEquipmentName","ResultIdentifier","ResultDetectionConditionText","MethodSpeciationName","CharacteristicName","ResultSampleFractionText","ResultMeasureValue","ResultMeasure/MeasureUnitCode",null,null,"MeasureQualifierCode","ResultStatusIdentifier","StatisticalBaseCode","ResultValueTypeName","ResultWeightBasisText","ResultTimeBasisText","ResultTemperatureBasisText","ResultParticleSizeBasisText","DataQuality/PrecisionValue","DataQuality/BiasValue","DataQuality/ConfidenceIntervalValue","DataQuality/UpperConfidenceLimitValue","DataQuality/LowerConfidenceLimitValue","ResultCommentText","USGSPCode","ResultDepthHeightMeasure/MeasureValue","ResultDepthHeightMeasure/MeasureUnitCode","ResultDepthAltitudeReferencePointText","SubjectTaxonomicName","SampleTissueAnatomyName","BinaryObjectFileName","BinaryObjectFileTypeCode","ResultFileUrl","ResultAnalyticalMethod/MethodIdentifier","ResultAnalyticalMethod/MethodIdentifierContext","ResultAnalyticalMethod/MethodName","ResultAnalyticalMethod/MethodUrl","ResultAnalyticalMethod/MethodDescriptionText","LaboratoryName","AnalysisStartDate","ResultLaboratoryCommentText","ResultDetectionQuantitationLimitUrl","DetectionQuantitationLimitTypeName","DetectionQuantitationLimitMeasure/MeasureValue","DetectionQuantitationLimitMeasure/MeasureUnitCode","LabSamplePreparationUrl","LastUpdated","ProviderName"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303448","Sample-Routine","Water","Surface Water","2012-11-19","10:25:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05485605",null,"L-3250012 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 101000  per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-OK","USGS Oklahoma Water Science Center","nwisok.01.01300353","Sample-Routine","Water","Surface Water","2012-11-28","11:37:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-07159735",null,"L-3340023 LC8285 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107222450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301736","Sample-Routine","Water","Surface Water","2012-12-05","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05373005",null,"L-3420030 X = LC8252 deleted per request from WSC Bode, PG, 12/7/12   Received December 06, 2012  Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235052","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300359","Sample-Routine","Water","Surface Water","2012-11-28","11:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01391100",null,"L-3340075 LC8252 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01306829","Sample-Routine","Water","Surface Water","2012-12-11","12:40:00","MST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394847104570700",null,"L-3470006 Updated time from 1230 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107243373","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303140","Sample-Routine","Water","Surface Water","2012-12-04","12:10:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-08057410",null,"L-3400056 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301741","Sample-Routine","Water","Surface Water","2012-12-04","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05340041",null,"L-3400039 Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235727","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01303146","Sample-Routine","Water","Surface Water","2012-11-19","13:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01421640",null,"L-3250019 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 133000 per Romanok.  KB 05/13/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107213401","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300361","Sample-Routine","Water","Surface Water","2012-12-10","12:10:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01409480",null,"L-3460046 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39777.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","11:31:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918138","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39777.CHEM/results/992918138/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39782.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","01:27:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918478","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39782.CHEM/results/992918478/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39774.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","12:04:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917934","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39774.CHEM/results/992917934/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39775.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","01:44:00","MST",{"$nulls":4},13.7,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62317",81818,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918002","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},13.7,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39775.CHEM/results/992918002/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39781.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","02:31:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918410","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39781.CHEM/results/992918410/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39787.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","02:15:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62315",81816,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918818","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39787.CHEM/results/992918818/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39762.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","02:43:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917118","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39762.CHEM/results/992917118/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39778.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","11:44:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918206","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39778.CHEM/results/992918206/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39763.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","12:07:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917186","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39763.CHEM/results/992917186/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39767.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","02:20:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62338",81835,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917458","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39767.CHEM/results/992917458/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39766.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","01:55:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917390","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39766.CHEM/results/992917390/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39779.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","01:07:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918274","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39779.CHEM/results/992918274/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39784.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","12:51:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62311",81812,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232588,-110.972266,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918614","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39784.CHEM/results/992918614/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39772.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","12:27:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917798","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39772.CHEM/results/992917798/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39788.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","12:52:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62333",81830,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918886","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39788.CHEM/results/992918886/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39769.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","01:36:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917594","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39769.CHEM/results/992917594/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39792.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","03:41:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62342",81839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992919158","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39792.CHEM/results/992919158/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39776.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","01:41:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918070","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39776.CHEM/results/992918070/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39771.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","02:08:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62337",81834,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917730","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39771.CHEM/results/992917730/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39780.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","12:22:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62318",81819,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918342","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39780.CHEM/results/992918342/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39768.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","10:56:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62322",81823,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917526","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39768.CHEM/results/992917526/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39790.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","12:33:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992919022","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39790.CHEM/results/992919022/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39773.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","01:57:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917866","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39773.CHEM/results/992917866/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39764.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","02:01:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62314",81815,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917254","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39764.CHEM/results/992917254/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39783.CHEM","Sample-Routine","Other","Groundwater","2022-08-08","11:09:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918546","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39783.CHEM/results/992918546/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39789.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","11:38:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918954","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39789.CHEM/results/992918954/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39785.CHEM","Sample-Routine","Other","Groundwater","2022-08-10","02:49:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992918682","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39785.CHEM/results/992918682/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39793.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","01:06:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62324",81825,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992919226","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39793.CHEM/results/992919226/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39770.CHEM","Sample-Routine","Other","Groundwater","2022-08-09","02:21:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992917662","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39770.CHEM/results/992917662/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:38:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43991.CHEM","Sample-Routine","Other","Groundwater","2023-01-25","01:38:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954880","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43991.CHEM/results/992954880/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43977.CHEM","Sample-Routine","Other","Groundwater","2023-02-08","03:33:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62550",81985,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006402,-110.159209,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992955220","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43977.CHEM/results/992955220/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43978.CHEM","Sample-Routine","Other","Groundwater","2023-02-08","04:25:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992955288","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43978.CHEM/results/992955288/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43976.CHEM","Sample-Routine","Other","Groundwater","2023-02-08","04:04:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992955152","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43976.CHEM/results/992955152/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43986.CHEM","Sample-Routine","Other","Groundwater","2023-01-25","12:32:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62550",81985,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006402,-110.159209,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954540","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43986.CHEM/results/992954540/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43989.CHEM","Sample-Routine","Other","Groundwater","2023-01-18","04:06:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62550",81985,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006402,-110.159209,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954744","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43989.CHEM/results/992954744/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43990.CHEM","Sample-Routine","Other","Groundwater","2023-01-18","04:50:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954812","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43990.CHEM/results/992954812/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43987.CHEM","Sample-Routine","Other","Groundwater","2023-01-18","05:28:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954608","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43987.CHEM/results/992954608/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43988.CHEM","Sample-Routine","Other","Groundwater","2023-01-25","12:54:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954676","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43988.CHEM/results/992954676/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43975.CHEM","Sample-Routine","Other","Groundwater","2023-02-08","03:49:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992955084","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43975.CHEM/results/992955084/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43993.CHEM","Sample-Routine","Other","Groundwater","2023-01-25","01:59:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992955016","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43993.CHEM/results/992955016/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43992.CHEM","Sample-Routine","Other","Groundwater","2023-01-18","04:23:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954948","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43992.CHEM/results/992954948/resdetectqntlmts","Laboratory Reporting Level",0.000104,"mg/m3",null,"2023-11-09T09:42:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30347.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","11:10:00","MST",{"$nulls":4},97.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47109",56731,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4256775,-111.9893181,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764448","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},97.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30347.CHEM/results/874764448/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30161.CHEM","Sample-Routine","Water","Groundwater","2020-10-31","03:10:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608061","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30161.CHEM/results/874608061/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30169.CHEM","Sample-Routine","Water","Groundwater","2020-11-01","11:35:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608653","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30169.CHEM/results/874608653/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30349.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","11:20:00","MST",{"$nulls":4},77.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47094",56714,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4257111,-111.9895264,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764596","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},77.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30349.CHEM/results/874764596/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30370.CHEM","Sample-Routine","Water","Groundwater","2020-11-12","10:30:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58666",79062,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5088167,-112.0496333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765561","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30370.CHEM/results/874765561/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30346.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","12:25:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47087",56706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4263119,-111.9909864,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764374","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30346.CHEM/results/874764374/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30369.CHEM","Sample-Routine","Water","Groundwater","2020-11-12","11:00:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62249",81752,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5038102,-112.0479517,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30369.CHEM/results/874765487/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29772.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","12:00:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29772.CHEM/results/871506378/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30348.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","01:15:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47103",56725,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4256089,-111.9923928,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764522","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30348.CHEM/results/874764522/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29778.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","04:30:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62483",81930,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4953,-112.00041,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506822","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29778.CHEM/results/871506822/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29773.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","02:05:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506452","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29773.CHEM/results/871506452/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30342.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","12:40:00","MST",{"$nulls":4},136,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47089",56708,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4256594,-111.9927419,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764078","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},136,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30342.CHEM/results/874764078/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30335.CHEM","Sample-Routine","Water","Groundwater","2020-10-30","11:35:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61657",81399,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.152385,-109.9742884,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874612594","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30335.CHEM/results/874612594/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T14:00:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30352.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","03:00:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47093",56713,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4261197,-111.9947167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764818","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30352.CHEM/results/874764818/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30351.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","01:00:00","MST",{"$nulls":4},88.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47098",56718,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4256475,-111.9925267,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764744","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},88.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30351.CHEM/results/874764744/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30167.CHEM","Sample-Routine","Water","Groundwater","2020-10-31","01:45:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59152",80430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1514111,-109.9719722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608505","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30167.CHEM/results/874608505/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30365.CHEM","Sample-Routine","Water","Groundwater","2020-11-12","09:00:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62248",81751,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5086333,-112.047725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765189","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30365.CHEM/results/874765189/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30339.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","11:40:00","MST",{"$nulls":4},72.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49556",56722,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4258625,-111.9903586,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874763856","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},72.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30339.CHEM/results/874763856/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30354.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","02:20:00","MST",{"$nulls":4},75,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47091",56711,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4266764,-111.9925761,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764966","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30354.CHEM/results/874764966/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29768.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","03:25:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58927",79646,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49344,-112.00216,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506082","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29768.CHEM/results/871506082/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29779.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","01:05:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29779.CHEM/results/871506896/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30337.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","10:30:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-42176",47718,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4256783,-111.9896886,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874763708","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30337.CHEM/results/874763708/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30340.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-11-16","08:00:00","MST",{"$nulls":4},72.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49556",56722,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4258625,-111.9903586,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874763930","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},72.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30340.CHEM/results/874763930/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30165.CHEM","Sample-Routine","Water","Groundwater","2020-10-30","03:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-6612",12173,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1508167,-109.97395,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30165.CHEM/results/874608357/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30164.CHEM","Sample-Routine","Water","Groundwater","2020-10-31","01:10:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61661",81403,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.152746,-109.9781317,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608283","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30164.CHEM/results/874608283/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29774.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","12:25:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506526","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29774.CHEM/results/871506526/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29770.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","02:55:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58931",79650,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4927,-112.00509,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506230","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29770.CHEM/results/871506230/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30334.CHEM","Sample-Routine","Water","Groundwater","2020-10-31","11:20:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874612520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30334.CHEM/results/874612520/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T14:00:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30363.CHEM","Sample-Routine","Water","Groundwater","2020-11-12","12:00:00","MST",{"$nulls":4},89,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58665",79061,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5095861,-112.0477528,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765040","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},89,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30363.CHEM/results/874765040/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30336.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-10-30","08:00:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874612668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30336.CHEM/results/874612668/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T14:00:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30345.CHEM","Sample-Routine","Water","Groundwater","2020-11-18","03:00:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47080",56696,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4254258,-112.0009269,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764300","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30345.CHEM/results/874764300/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30168.CHEM","Sample-Routine","Water","Groundwater","2020-10-31","02:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30168.CHEM/results/874608579/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30163.CHEM","Sample-Routine","Water","Groundwater","2020-11-02","06:15:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59149",80427,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1545417,-109.9757,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608209","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30163.CHEM/results/874608209/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29771.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","03:55:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62234",81738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4949968,-112.0012566,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29771.CHEM/results/871506304/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30341.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","12:00:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47095",56715,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4258625,-111.9903586,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L2,R5,.",null,110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30341.CHEM/results/874764004/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29769.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-10-09","08:00:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29769.CHEM/results/871506156/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29767.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","01:45:00","MST",{"$nulls":4},118,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-40409",46727,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49439,-112.00447,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506008","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},118,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29767.CHEM/results/871506008/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30344.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","02:00:00","MST",{"$nulls":4},120,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49441",59328,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4268958,-111.9956719,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764226","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},120,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30344.CHEM/results/874764226/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30343.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","10:35:00","MST",{"$nulls":4},92.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-45636",47717,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.42565,-111.9895978,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},92.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30343.CHEM/results/874764152/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30159.CHEM","Sample-Routine","Water","Groundwater","2020-10-31","11:10:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874607913","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30159.CHEM/results/874607913/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:56:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30162.CHEM","Sample-Routine","Water","Groundwater","2020-10-30","04:55:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30162.CHEM/results/874608135/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30160.CHEM","Sample-Routine","Water","Groundwater","2020-11-03","12:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874607987","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30160.CHEM/results/874607987/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:56:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30368.CHEM","Sample-Routine","Water","Groundwater","2020-11-12","08:30:00","MST",{"$nulls":4},125,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61764",81459,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5088601,-112.0540506,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765413","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},125,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30368.CHEM/results/874765413/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29777.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","11:30:00","MST",{"$nulls":4},117,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54635",62158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.00218,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},117,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29777.CHEM/results/871506748/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29776.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","01:20:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29776.CHEM/results/871506674/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30338.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-11-16","08:05:00","MST",{"$nulls":4},88.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47098",56718,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4256475,-111.9925267,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874763782","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},88.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30338.CHEM/results/874763782/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:51:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30353.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","03:30:00","MST",{"$nulls":4},89,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47084",56701,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4235719,-111.9955856,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764892","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},89,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30353.CHEM/results/874764892/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30350.CHEM","Sample-Routine","Water","Groundwater","2020-11-16","10:45:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47085",56702,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4256869,-111.9896175,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874764670","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30350.CHEM/results/874764670/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-02-04T10:52:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30333.CHEM","Sample-Routine","Water","Groundwater","2020-10-31","12:20:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43884",49649,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498085,-109.9734159,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874612446","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30333.CHEM/results/874612446/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T14:00:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30166.CHEM","Sample-Routine","Water","Groundwater","2020-10-30","04:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61656",81398,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.150759,-109.9739609,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874608431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30166.CHEM/results/874608431/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2021-01-29T13:57:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29775.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","02:30:00","MST",{"$nulls":4},216,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61627",81371,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49253,-112.00725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506600","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},216,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29775.CHEM/results/871506600/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2020-12-30T18:52:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44891.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","07:44:00","MST",{"$nulls":4},83,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974185265","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},83,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44891.CHEM/results/974185265/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:04:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44895.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","08:04:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974185578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44895.CHEM/results/974185578/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:05:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44930.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-06-02","12:00:00","MST",{"$nulls":4},83,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974188282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},83,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44930.CHEM/results/974188282/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:09:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44908.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","10:05:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974186585","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44908.CHEM/results/974186585/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:06:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44889.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","08:23:00","MST",{"$nulls":4},93,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974185110","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},93,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44889.CHEM/results/974185110/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:04:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44888.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","09:46:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974185034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44888.CHEM/results/974185034/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:04:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44913.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","11:37:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974186974","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44913.CHEM/results/974186974/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:07:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44874.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","10:42:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974183952","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44874.CHEM/results/974183952/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:02:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44890.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","08:41:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974185189","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44890.CHEM/results/974185189/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:04:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44887.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","11:01:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974184957","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44887.CHEM/results/974184957/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:04:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44871.CHEM","Sample-Routine","Water","Groundwater","2021-06-02","10:24:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974183711","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44871.CHEM/results/974183711/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-05-05T10:02:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37454.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","09:49:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49518",59451,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.508745,-112.0739306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901395","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37454.CHEM/results/992901395/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37445.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","05:50:00","MST",{"$nulls":4},350,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62804",82183,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5147024,-112.0742958,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},350,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37445.CHEM/results/992900729/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37461.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","09:15:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-57301",74220,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5146417,-112.0740333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901913","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37461.CHEM/results/992901913/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37467.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","06:54:00","MST",{"$nulls":4},180,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62692",82097,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5083552,-112.0731066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},180,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37467.CHEM/results/992902357/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37458.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","05:15:00","MST",{"$nulls":4},190,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-51853",59449,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089639,-112.0741806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901691","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},190,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37458.CHEM/results/992901691/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37470.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","05:40:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49517",59450,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089358,-112.0742047,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37470.CHEM/results/992902579/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37472.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-04-06","12:00:00","MST",{"$nulls":4},350,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62804",82183,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5147024,-112.0742958,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902727","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},350,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37472.CHEM/results/992902727/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37456.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","01:22:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50271",60374,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089417,-112.0739917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901543","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37456.CHEM/results/992901543/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37449.CHEM","Sample-Routine","Water","Groundwater","2022-04-08","02:30:00","MST",{"$nulls":4},83,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55120",67539,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5082847,-112.0739647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901025","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},83,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37449.CHEM/results/992901025/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37465.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","12:36:00","MST",{"$nulls":4},81,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55118",67537,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5117814,-112.0741767,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902209","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},81,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37465.CHEM/results/992902209/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37464.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-04-06","12:00:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49518",59451,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.508745,-112.0739306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37464.CHEM/results/992902135/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37471.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","12:00:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50272",60375,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5087536,-112.0739797,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902653","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37471.CHEM/results/992902653/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37452.CHEM","Sample-Routine","Water","Groundwater","2022-04-08","01:20:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55124",67543,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5090942,-112.0743069,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901247","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37452.CHEM/results/992901247/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37468.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","11:57:00","MST",{"$nulls":4},81,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58628",78968,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5112,-112.0728639,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},81,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37468.CHEM/results/992902431/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37457.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","06:30:00","MST",{"$nulls":4},172,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62805",82184,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5147024,-112.074295,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901617","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},172,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37457.CHEM/results/992901617/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37446.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","01:20:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54184",61809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5104497,-112.0743658,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37446.CHEM/results/992900803/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37469.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","11:25:00","MST",{"$nulls":4},84,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58629",78969,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5111917,-112.0715472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902505","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},84,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37469.CHEM/results/992902505/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37448.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","08:18:00","MST",{"$nulls":4},75,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-57302",74221,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5099694,-112.0728806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900951","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37448.CHEM/results/992900951/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37444.CHEM","Sample-Routine","Water","Groundwater","2022-04-08","03:06:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55484",68458,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5074672,-112.07421,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37444.CHEM/results/992900655/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37450.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","02:53:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50270",60373,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5090111,-112.0739639,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901099","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37450.CHEM/results/992901099/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37466.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","05:34:00","MST",{"$nulls":4},330,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62804",82183,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5147024,-112.0742958,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902283","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},330,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37466.CHEM/results/992902283/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37462.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","10:47:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50273",60376,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5085703,-112.0739794,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901987","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37462.CHEM/results/992901987/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37459.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","01:58:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54183",61808,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5098447,-112.0745547,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901765","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37459.CHEM/results/992901765/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37453.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","04:32:00","MST",{"$nulls":4},292,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49516",59448,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089208,-112.0741147,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},292,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37453.CHEM/results/992901321/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37455.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","06:14:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62693",82098,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5083554,-112.0731057,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992901469","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37455.CHEM/results/992901469/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37463.CHEM","Sample-Routine","Water","Groundwater","2022-04-08","04:47:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-53680",64596,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5086864,-112.0743511,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902061","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37463.CHEM/results/992902061/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37447.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","08:58:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62802",82181,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5086378,-112.0724669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900877","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37447.CHEM/results/992900877/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",null,"2023-11-09T09:37:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47504.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","10:35:00","MST",{"$nulls":4},170,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48042",57710,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2298717,-111.3358622,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986325","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},170,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47504.CHEM/results/992986325/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47501.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","09:30:00","MST",{"$nulls":4},280,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48054",57722,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2294514,-111.3268761,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986082","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},280,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47501.CHEM/results/992986082/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47512.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","01:00:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-49044",58917,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2445478,-111.3361836,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986968","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47512.CHEM/results/992986968/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47506.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","09:15:00","MST",{"$nulls":4},180,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48053",57721,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2294356,-111.3268981,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},180,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47506.CHEM/results/992986487/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47500.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","11:05:00","MST",{"$nulls":4},93.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59324",81026,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2291719,-111.3275581,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999651787","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},93.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47500.CHEM/results/999651787/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2024-01-18T09:30:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47509.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","12:30:00","MST",{"$nulls":4},180,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-47053",56667,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2287586,-111.3285047,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986724","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},180,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47509.CHEM/results/992986724/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47508.CHEM","Quality Control Sample-Equipment Blank","Water","Groundwater","2022-04-17","12:00:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48054",57722,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2294514,-111.3268761,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986644","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47508.CHEM/results/992986644/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47507.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","11:30:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59326",81028,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2290539,-111.3274094,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999651869","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47507.CHEM/results/999651869/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2024-01-18T09:30:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47502.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","10:00:00","MST",{"$nulls":4},230,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48036",57704,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2285256,-111.3335314,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},230,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47502.CHEM/results/992986163/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47510.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","01:25:00","MST",{"$nulls":4},70,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-51864",59470,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2293192,-111.3296236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986805","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},70,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47510.CHEM/results/992986805/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47511.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","12:00:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59329",81031,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2290775,-111.3276856,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999651951","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47511.CHEM/results/999651951/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2024-01-18T09:30:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47503.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","01:40:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-49536",59471,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2293383,-111.3297047,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47503.CHEM/results/992986244/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47505.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","12:45:00","MST",{"$nulls":4},117,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-47147",56666,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2287419,-111.3285278,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986406","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},117,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47505.CHEM/results/992986406/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",null,"2023-11-09T09:45:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30382.CHEM","Sample-Routine","Water","Groundwater","2017-12-08","11:17:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43884",49649,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498085,-109.9734159,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874904105","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30382.CHEM/results/874904105/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:52","STORET"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303450","Sample-Routine","Water","Surface Water","2013-05-20","12:15:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05451210",null,"L-1410060 Evn. ASR & smpls changed to 1215 per K.Romanok, paa, 5/21/13..  LC8252 deleted per Rose, paa, 5/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30383.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2017-12-07","06:47:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874904179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30383.CHEM/results/874904179/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30384.CHEM","Sample-Routine","Water","Groundwater","2017-12-07","06:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874904253","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30384.CHEM/results/874904253/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30381.CHEM","Sample-Routine","Water","Groundwater","2018-11-16","04:35:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43884",49649,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498085,-109.9734159,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874904031","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30381.CHEM/results/874904031/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30379.CHEM","Sample-Routine","Water","Groundwater","2018-11-16","04:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903883","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30379.CHEM/results/874903883/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18670.CHEM","Sample-Routine","Water","Groundwater","2018-11-13","02:40:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61661",81403,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.152746,-109.9781317,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18670.CHEM/results/789184211/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18599.CHEM","Sample-Routine","Water","Groundwater","2018-06-25","05:55:00","EST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61648",81391,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.515908,-112.0651612,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789230698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18599.CHEM/results/789230698/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-13T09:47:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30380.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2018-11-16","01:25:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903957","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30380.CHEM/results/874903957/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18662.CHEM","Sample-Routine","Water","Groundwater","2018-11-16","08:55:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184581","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18662.CHEM/results/789184581/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18668.CHEM","Sample-Routine","Water","Groundwater","2018-11-13","04:05:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184359","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18668.CHEM/results/789184359/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18659.CHEM","Sample-Routine","Water","Groundwater","2018-11-16","02:47:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184285","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18659.CHEM/results/789184285/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18669.CHEM","Sample-Routine","Water","Groundwater","2018-11-13","11:30:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183693","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18669.CHEM/results/789183693/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18666.CHEM","Sample-Routine","Water","Groundwater","2018-11-15","06:10:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61655",81397,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1498278,-109.9722806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184063","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18666.CHEM/results/789184063/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18600.CHEM","Sample-Routine","Water","Groundwater","2018-06-25","03:55:00","EST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58634",78974,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.5163472,-112.0651667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789230550","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18600.CHEM/results/789230550/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-13T09:47:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18667.CHEM","Sample-Routine","Water","Groundwater","2018-11-14","04:05:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61658",81400,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.15071,-109.9747382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18667.CHEM/results/789183915/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18663.CHEM","Sample-Routine","Water","Groundwater","2018-11-15","10:15:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18663.CHEM/results/789183767/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18660.CHEM","Sample-Routine","Water","Groundwater","2018-11-16","04:55:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183989","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18660.CHEM/results/789183989/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18601.CHEM","Sample-Routine","Water","Groundwater","2018-06-25","01:25:00","EST",{"$nulls":4},91,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58633",78973,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.5152806,-112.0659583,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789230624","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},91,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18601.CHEM/results/789230624/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-13T09:47:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18661.CHEM","Sample-Routine","Water","Groundwater","2018-11-14","04:55:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-6612",12173,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1508167,-109.97395,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184137","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18661.CHEM/results/789184137/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18664.CHEM","Sample-Routine","Water","Groundwater","2018-11-16","01:05:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59152",80430,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1514111,-109.9719722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184433","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18664.CHEM/results/789184433/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18655.CHEM","Sample-Routine","Water","Groundwater","2018-07-30","02:40:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-788805139","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18655.CHEM/results/788805139/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-07T09:21:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18665.CHEM","Sample-Routine","Water","Groundwater","2018-11-14","04:28:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61656",81398,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.150759,-109.9739609,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183841","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18665.CHEM/results/789183841/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18671.CHEM","Sample-Routine","Water","Groundwater","2018-11-16","10:35:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59149",80427,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1545417,-109.9757,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184507","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18671.CHEM/results/789184507/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28085.CHEM","Sample-Routine","Water","Groundwater","2019-12-02","02:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59152",80430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1514111,-109.9719722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804364","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28085.CHEM/results/849804364/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18709.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","01:00:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59152",80430,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1514111,-109.9719722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185173","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18709.CHEM/results/789185173/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28078.CHEM","Sample-Routine","Water","Groundwater","2019-12-02","10:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849803846","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28078.CHEM/results/849803846/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30375.CHEM","Sample-Routine","Water","Groundwater","2019-12-01","03:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903735","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30375.CHEM/results/874903735/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28079.CHEM","Sample-Routine","Water","Groundwater","2019-12-01","04:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849803920","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28079.CHEM/results/849803920/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18707.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","10:00:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185469","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18707.CHEM/results/789185469/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18715.CHEM","Sample-Routine","Water","Groundwater","2019-04-29","03:00:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61656",81398,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.150759,-109.9739609,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18715.CHEM/results/789184655/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18706.CHEM","Sample-Routine","Water","Groundwater","2019-04-29","06:30:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61655",81397,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1498278,-109.9722806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185025","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18706.CHEM/results/789185025/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18711.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","07:45:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61661",81403,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.152746,-109.9781317,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185099","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18711.CHEM/results/789185099/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30376.CHEM","Sample-Routine","Water","Groundwater","2019-12-02","12:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43884",49649,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498085,-109.9734159,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903809","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30376.CHEM/results/874903809/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28077.CHEM","Sample-Routine","Water","Groundwater","2019-12-03","11:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59149",80427,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1545417,-109.9757,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849803772","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28077.CHEM/results/849803772/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18714.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","07:10:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185617","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18714.CHEM/results/789185617/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18713.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","09:35:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59149",80427,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1545417,-109.9757,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184951","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18713.CHEM/results/789184951/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28083.CHEM","Sample-Routine","Water","Groundwater","2019-12-02","03:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-6612",12173,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1508167,-109.97395,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28083.CHEM/results/849804216/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18716.CHEM","Sample-Routine","Water","Groundwater","2019-04-29","04:35:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185395","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18716.CHEM/results/789185395/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18712.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2019-04-30","06:00:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18712.CHEM/results/789184803/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30378.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","02:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43884",49649,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498085,-109.9734159,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903587","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30378.CHEM/results/874903587/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28090.CHEM","Sample-Routine","Water","Groundwater","2019-12-02","03:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61656",81398,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.150759,-109.9739609,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804734","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28090.CHEM/results/849804734/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28075.CHEM","Sample-Routine","Water","Groundwater","2019-12-01","05:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61661",81403,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.152746,-109.9781317,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849803624","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28075.CHEM/results/849803624/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28082.CHEM","Sample-Routine","Water","Groundwater","2019-12-01","03:55:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61655",81397,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498278,-109.9722806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28082.CHEM/results/849804142/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18704.CHEM","Sample-Routine","Water","Groundwater","2019-04-29","01:10:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61658",81400,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.15071,-109.9747382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185543","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18704.CHEM/results/789185543/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18708.CHEM","Sample-Routine","Water","Groundwater","2019-04-29","03:45:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-6612",12173,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1508167,-109.97395,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185247","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18708.CHEM/results/789185247/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28088.CHEM","Sample-Routine","Water","Groundwater","2019-12-01","06:10:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804586","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28088.CHEM/results/849804586/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28081.CHEM","Sample-Routine","Water","Groundwater","2019-12-03","10:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804068","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28081.CHEM/results/849804068/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28084.CHEM","Sample-Routine","Water","Groundwater","2019-12-03","10:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804290","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28084.CHEM/results/849804290/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18710.CHEM","Sample-Routine","Water","Groundwater","2019-04-29","01:30:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18710.CHEM/results/789184729/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30374.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2019-12-03","06:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903661","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30374.CHEM/results/874903661/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28076.CHEM","Sample-Routine","Water","Groundwater","2019-12-02","09:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61658",81400,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.15071,-109.9747382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849803698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28076.CHEM/results/849803698/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28086.CHEM","Sample-Routine","Water","Groundwater","2019-12-01","02:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804438","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28086.CHEM/results/849804438/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28087.CHEM","Sample-Routine","Water","Groundwater","2019-12-03","11:15:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804512","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28087.CHEM/results/849804512/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18705.CHEM","Sample-Routine","Water","Groundwater","2019-04-30","09:00:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789185321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18705.CHEM/results/789185321/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18703.CHEM","Sample-Routine","Water","Groundwater","2019-05-01","08:30:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184877","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18703.CHEM/results/789184877/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-06-12T10:04:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30377.CHEM","Sample-Routine","Water","Groundwater","2019-04-29","07:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903513","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30377.CHEM/results/874903513/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-05T12:53:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28089.CHEM","Sample-Routine","Water","Groundwater","2019-12-03","11:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28089.CHEM/results/849804660/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28080.CHEM","Sample-Routine","Water","Groundwater","2019-12-02","11:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849803994","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28080.CHEM/results/849803994/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28312.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","04:15:00","MST",{"$nulls":4},82,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55119",67538,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5119953,-112.0729422,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122134","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},82,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28312.CHEM/results/850122134/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28101.CHEM","Sample-Routine","Water","Groundwater","2020-04-05","10:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805622","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28101.CHEM/results/849805622/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28315.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","10:55:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49518",59451,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.508745,-112.0739306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122356","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28315.CHEM/results/850122356/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28317.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-03-27","08:00:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50273",60376,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5085703,-112.0739794,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122504","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28317.CHEM/results/850122504/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28324.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","03:50:00","MST",{"$nulls":4},84,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58629",78969,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5111917,-112.0715472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},84,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28324.CHEM/results/850123022/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28095.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","11:05:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61658",81400,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.15071,-109.9747382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805104","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28095.CHEM/results/849805104/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28093.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","11:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61658",81400,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.15071,-109.9747382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804956","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28093.CHEM/results/849804956/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28109.CHEM","Sample-Routine","Water","Groundwater","2020-04-02","05:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-35863",46085,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0852919,-114.6020647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849876229","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28109.CHEM/results/849876229/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-24T11:03:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28330.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","12:20:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54184",61809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5104497,-112.0743658,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123466","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28330.CHEM/results/850123466/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:17:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28322.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","01:15:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55484",68458,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5074672,-112.07421,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122874","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28322.CHEM/results/850122874/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28316.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","03:15:00","MST",{"$nulls":4},75,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-57302",74221,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5099694,-112.0728806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122430","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28316.CHEM/results/850122430/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28313.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","11:35:00","MST",{"$nulls":4},292,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49516",59448,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089208,-112.0741147,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122208","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},292,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28313.CHEM/results/850122208/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28107.CHEM","Sample-Routine","Water","Groundwater","2020-04-01","11:20:00","MST",{"$nulls":4},35,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-39781",46087,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0761556,-114.5983,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849876154","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},35,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28107.CHEM/results/849876154/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-24T11:03:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28104.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","11:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-6612",12173,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1508167,-109.97395,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805844","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28104.CHEM/results/849805844/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28092.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","12:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804882","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28092.CHEM/results/849804882/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28103.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","12:10:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805770","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28103.CHEM/results/849805770/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28091.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","11:40:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804808","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28091.CHEM/results/849804808/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28328.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","03:35:00","MST",{"$nulls":4},81,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58628",78968,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5112,-112.0728639,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},81,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28328.CHEM/results/850123318/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:17:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28329.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-03-26","08:00:00","MST",{"$nulls":4},75,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-57302",74221,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5099694,-112.0728806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123392","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: M1.",null,75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28329.CHEM/results/850123392/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:17:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28321.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","01:45:00","MST",{"$nulls":4},83,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55120",67539,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5082847,-112.0739647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122800","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},83,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28321.CHEM/results/850122800/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28327.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","12:05:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49517",59450,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089358,-112.0742047,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28327.CHEM/results/850123244/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:17:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28106.CHEM","Sample-Routine","Water","Groundwater","2020-04-01","11:40:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-39780",46086,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0762236,-114.5983106,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849876081","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28106.CHEM/results/849876081/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-24T11:03:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28331.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","09:45:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50270",60373,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5090111,-112.0739639,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123540","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28331.CHEM/results/850123540/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:17:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28102.CHEM","Sample-Routine","Water","Groundwater","2020-04-05","01:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805696","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28102.CHEM/results/849805696/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28333.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","02:05:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-53680",64596,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5086864,-112.0743511,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123688","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28333.CHEM/results/850123688/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:17:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28318.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","10:25:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50271",60374,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089417,-112.0739917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28318.CHEM/results/850122578/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28098.CHEM","Sample-Routine","Water","Groundwater","2020-04-05","11:30:00","MST",{"$nulls":4},50,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61655",81397,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498278,-109.9722806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},50,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28098.CHEM/results/849805326/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28097.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","11:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61656",81398,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.150759,-109.9739609,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805252","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28097.CHEM/results/849805252/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28326.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","10:40:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50272",60375,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5087536,-112.0739797,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123170","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28326.CHEM/results/850123170/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28096.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","02:05:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59149",80427,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1545417,-109.9757,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805178","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},45,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28096.CHEM/results/849805178/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28100.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","10:05:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805543","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28100.CHEM/results/849805543/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28314.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","11:20:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-57301",74220,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5146417,-112.0740333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28314.CHEM/results/850122282/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30372.CHEM","Sample-Routine","Water","Groundwater","2020-04-05","12:00:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43884",49649,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1498085,-109.9734159,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765709","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30372.CHEM/results/874765709/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-04T10:52:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28100.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","10:05:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28100.CHEM/results/849805544/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28105.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","01:10:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59152",80430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1514111,-109.9719722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805918","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28105.CHEM/results/849805918/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28320.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","11:50:00","MST",{"$nulls":4},81,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55118",67537,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5117814,-112.0741767,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},81,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28320.CHEM/results/850122726/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28325.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","11:15:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50273",60376,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5085703,-112.0739794,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123096","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28325.CHEM/results/850123096/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30373.CHEM","Sample-Routine","Water","Groundwater","2020-04-05","11:00:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765783","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30373.CHEM/results/874765783/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-04T10:52:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28332.CHEM","Sample-Routine","Water","Groundwater","2020-03-26","12:40:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54183",61808,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5098447,-112.0745547,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123614","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28332.CHEM/results/850123614/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:17:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30371.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-04-05","08:00:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765635","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30371.CHEM/results/874765635/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2021-02-04T10:52:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28099.CHEM","Sample-Routine","Water","Groundwater","2020-04-05","12:25:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61661",81403,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.152746,-109.9781317,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805400","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28099.CHEM/results/849805400/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28319.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","12:25:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-55124",67543,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5090942,-112.0743069,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122652","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28319.CHEM/results/850122652/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28311.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","11:55:00","MST",{"$nulls":4},190,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-51853",59449,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089639,-112.0741806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122060","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},190,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28311.CHEM/results/850122060/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-07-06T11:16:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28094.CHEM","Sample-Routine","Water","Groundwater","2020-04-05","12:50:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849805030","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28094.CHEM/results/849805030/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2020-06-22T11:29:25","STORET"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01301526","Sample-Routine","Water","Surface Water","2013-05-13","11:40:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-324305097101900",null,"L-1350041 Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28323.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","09:25:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50269",60372,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5090444,-112.0739778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850122948","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28323.CHEM/results/850122948/resdetectqntlmts","Laboratory Reporting Level",1.65E-3,"mg/L",null,"2020-07-06T11:16:57","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132074-gwdb","Sample-Routine","Water","Groundwater","2012-12-27","10:52:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79222","ADEQ MW-102",{"$nulls":4},32.2461081,-109.8364322,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491400933","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2012-12-30",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132074-gwdb/results/491400933/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-12-01T14:17:26","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132072-gwdb","Sample-Routine","Water","Groundwater","2012-12-27","10:36:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491394713","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2012-12-30",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132072-gwdb/results/491394713/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-12-01T14:15:07","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122643-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","08:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122643-gwdb/results/490882282/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:12:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120461R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","09:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490941363","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120461R-gwdb/results/490941363/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:50","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120296R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","08:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490940315","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120296R-gwdb/results/490940315/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:23","STORET"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301372","Sample-Routine","Water","Surface Water","2013-03-12","15:20:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02281200",null,"L-0730004 Updated time from 1500 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107230079","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-03-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132039-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","16:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79223","ADEQ MW-103",{"$nulls":4},32.2459961,-109.8361039,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490960861","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132039-gwdb/results/490960861/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:13","STORET"]
["USGS-PR","USGS Puerto Rico Water Science Center","nwispr.01.01301107","Sample-Routine","Water","Surface Water","2013-03-19","10:40:00","AST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-50055410",null,"L-0790103 Updated time from 103000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107219605","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-03","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132037-gwdb","Sample-Routine","Water","Groundwater","2013-09-11","09:25:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882710","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":9},"Qualifier:   DUPLICATES:  MS/MSD RPD EXCEEDED THE LABORATORY CONTROL ACCEPTANCE LIMIT. RECOVERY MET ACCEPTANCE CRITERIA.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-15",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132037-gwdb/results/490882710/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:12:41","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120462R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","09:35:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490947676","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120462R-gwdb/results/490947676/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:43:13","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120526R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","11:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491006777","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120526R-gwdb/results/491006777/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:11:49","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120445R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","10:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490941445","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120445R-gwdb/results/490941445/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:51","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122650-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","07:25:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490895819","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122650-gwdb/results/490895819/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:20:22","STORET"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302619","Sample-Routine","Water","Surface Water","2013-04-16","10:10:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02335870",null,"L-1080111 Received April 17, 2013  Updated time from 100000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107221194","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122692-gwdb","Sample-Routine","Water","Groundwater","2013-04-08","09:07:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79223","ADEQ MW-103",{"$nulls":4},32.2459961,-109.8361039,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490885237","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-04-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122692-gwdb/results/490885237/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:14:24","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132036-gwdb","Sample-Routine","Water","Groundwater","2013-09-11","08:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962525","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132036-gwdb/results/490962525/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:42","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132027-gwdb","Sample-Routine","Water","Groundwater","2013-09-11","06:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79222","ADEQ MW-102",{"$nulls":4},32.2461081,-109.8364322,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490960944","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132027-gwdb/results/490960944/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:15","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122570-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","06:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490884624","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122570-gwdb/results/490884624/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:14:01","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132033-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","11:45:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490885462","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132033-gwdb/results/490885462/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:14:32","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132347-gwdb","Sample-Routine","Water","Groundwater","2013-05-21","09:42:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79541","ADEQ MW-1A",{"$nulls":4},32.2267986,-110.967605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490961476","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-05-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132347-gwdb/results/490961476/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120527R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","11:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490866362","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120527R-gwdb/results/490866362/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:58:16","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120289R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","11:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490768011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120289R-gwdb/results/490768011/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:47:24","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122642-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","08:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490809263","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122642-gwdb/results/490809263/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:19:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120359R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","07:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120359R-gwdb/results/490802011/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:14:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122648-gwdb","Sample-Routine","Water","Groundwater","2013-12-16","12:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490809437","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122648-gwdb/results/490809437/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:19:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122567-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","16:20:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490884603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122567-gwdb/results/490884603/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:14:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120496R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","10:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490941537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120496R-gwdb/results/490941537/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:53","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122696-gwdb","Sample-Routine","Water","Groundwater","2013-04-08","10:28:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490775493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-04-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122696-gwdb/results/490775493/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:50:59","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122649-gwdb","Sample-Routine","Water","Groundwater","2013-12-16","13:35:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490961983","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122649-gwdb/results/490961983/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:33","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120497R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","10:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491006715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120497R-gwdb/results/491006715/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:11:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122644-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","09:20:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490960756","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122644-gwdb/results/490960756/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122694-gwdb","Sample-Routine","Water","Groundwater","2013-04-08","09:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490885380","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-04-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122694-gwdb/results/490885380/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:14:30","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132029-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","10:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962275","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132029-gwdb/results/490962275/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:36","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122657-gwdb","Sample-Routine","Water","Groundwater","2013-12-16","13:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882454","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122657-gwdb/results/490882454/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:12:27","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120525R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","10:35:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490947757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120525R-gwdb/results/490947757/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:43:14","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122688-gwdb","Sample-Routine","Water","Groundwater","2013-08-12","11:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962061","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122688-gwdb/results/490962061/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:33","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120288R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","11:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491003426","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120288R-gwdb/results/491003426/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:09:42","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120495R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","09:40:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769287","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120495R-gwdb/results/490769287/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:48:01","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120524R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","10:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490862524","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120524R-gwdb/results/490862524/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:55:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120508R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","11:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491004622","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120508R-gwdb/results/491004622/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:10:23","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132024-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","12:40:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490775599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132024-gwdb/results/490775599/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:51:02","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132032-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490775503","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132032-gwdb/results/490775503/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:51:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122699-gwdb","Sample-Routine","Water","Groundwater","2013-05-09","11:40:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962238","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-05-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122699-gwdb/results/490962238/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:36","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122568-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","13:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79264","ADEQ MW-104",{"$nulls":4},32.2674414,-109.8470308,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490877640","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122568-gwdb/results/490877640/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:07:57","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122654-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","08:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490893513","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122654-gwdb/results/490893513/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:19:13","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122571-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","14:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79265","ADEQ MW-105",{"$nulls":4},32.2671364,-109.8474781,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490774872","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122571-gwdb/results/490774872/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:50:38","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132352-gwdb","Sample-Routine","Water","Groundwater","2013-05-21","09:36:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79541","ADEQ MW-1A",{"$nulls":4},32.2267986,-110.967605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-05-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132352-gwdb/results/490962821/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:45","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122698-gwdb","Sample-Routine","Water","Groundwater","2013-04-08","10:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490775283","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-04-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122698-gwdb/results/490775283/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:50:52","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132031-gwdb","Sample-Routine","Water","Groundwater","2013-09-11","12:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490893729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-15",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132031-gwdb/results/490893729/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:19:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122685-gwdb","Sample-Routine","Water","Groundwater","2013-08-12","11:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962112","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122685-gwdb/results/490962112/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122566-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","12:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79263","ADEQ MW-103",{"$nulls":4},32.2673994,-109.8469225,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490774755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122566-gwdb/results/490774755/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:50:35","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120319R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","08:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802056","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120319R-gwdb/results/490802056/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:14:58","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132026-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","15:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882581","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132026-gwdb/results/490882581/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:12:36","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120523R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","10:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490862437","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120523R-gwdb/results/490862437/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:55:44","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122686-gwdb","Sample-Routine","Water","Groundwater","2013-08-12","11:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490895893","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122686-gwdb/results/490895893/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:20:23","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122687-gwdb","Sample-Routine","Water","Groundwater","2013-08-12","10:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882571","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122687-gwdb/results/490882571/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:12:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122569-gwdb","Sample-Routine","Water","Groundwater","2013-12-17","15:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79262","ADEQ MW-102",{"$nulls":4},32.26686,-109.8468753,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490884469","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122569-gwdb/results/490884469/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:13:57","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132376-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","14:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79541","ADEQ MW-1A",{"$nulls":4},32.2267986,-110.967605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490961647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132376-gwdb/results/490961647/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120410R-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","08:58:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490865821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120410R-gwdb/results/490865821/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:58:00","STORET"]
["USGS-NE","USGS Nebraska Water Science Center","nwisne.01.01300271","Sample-Routine","Water","Surface Water","2013-06-10","10:10:00","CDT",{"$nulls":14},"USGS-06770195",null,"L-1640193 Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120313R-gwdb","Sample-Routine","Water","Groundwater","2014-05-19","07:33:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65607","ADEQ MW-7",{"$nulls":4},33.5275464,-112.0812694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802257","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120313R-gwdb/results/490802257/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:05","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122412-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","12:45:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79264","ADEQ MW-104",{"$nulls":4},32.2674414,-109.8470308,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490960200","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122412-gwdb/results/490960200/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:48:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132469-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","11:22:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490811459","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132469-gwdb/results/490811459/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132363-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","11:23:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79543","ADEQ MW-4",{"$nulls":4},32.2265778,-110.9674953,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490810023","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132363-gwdb/results/490810023/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122444-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","09:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490808258","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122444-gwdb/results/490808258/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:19:02","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121780-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","12:58:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491008223","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121780-gwdb/results/491008223/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:12:42","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122423-gwdb","Sample-Routine","Water","Groundwater","2014-05-20","16:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490877001","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122423-gwdb/results/490877001/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:07:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132481-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","10:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490828732","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132481-gwdb/results/490828732/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:32:31","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132465-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","13:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79222","ADEQ MW-102",{"$nulls":4},32.2461081,-109.8364322,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490889869","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132465-gwdb/results/490889869/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:17:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132371-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","09:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79544","ADEQ MW-9",{"$nulls":4},32.2270219,-110.9675036,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490897313","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132371-gwdb/results/490897313/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:21:11","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120333R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","09:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490942682","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-01-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120333R-gwdb/results/490942682/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:41:31","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122451-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","10:16:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490774327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122451-gwdb/results/490774327/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:50:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122441-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","08:37:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491018159","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122441-gwdb/results/491018159/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120440R-gwdb","Sample-Routine","Water","Groundwater","2014-03-18","13:08:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79329","ADEQ MW-19",{"$nulls":4},33.5262031,-112.0829206,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490941034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120440R-gwdb/results/490941034/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132377-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","18:45:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-57557","YELLOW CAB MW YC-6",{"$nulls":4},32.2262906,-110.968795,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490897326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132377-gwdb/results/490897326/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:21:12","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132471-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","10:03:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490964890","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132471-gwdb/results/490964890/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:50:32","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120465R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490862621","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120465R-gwdb/results/490862621/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:55:52","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122406-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","15:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79263","ADEQ MW-103",{"$nulls":4},32.2673994,-109.8469225,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490876950","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122406-gwdb/results/490876950/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:07:08","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120500R-gwdb","Sample-Other","Water","Groundwater","2014-03-20","08:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490803281","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120500R-gwdb/results/490803281/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132479-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","13:20:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490811347","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132479-gwdb/results/490811347/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:54","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122413-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","16:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017630","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122413-gwdb/results/491017630/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:33","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132381-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","14:45:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79541","ADEQ MW-1A",{"$nulls":4},32.2267986,-110.967605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490810304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132381-gwdb/results/490810304/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:17","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121775-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","08:21:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490946349","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121775-gwdb/results/490946349/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:42:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122435-gwdb","Sample-Routine","Water","Groundwater","2014-09-24","11:44:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490880201","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122435-gwdb/results/490880201/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:10:08","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122427-gwdb","Sample-Routine","Water","Groundwater","2014-09-25","10:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79222","ADEQ MW-102",{"$nulls":4},32.2461081,-109.8364322,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017863","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122427-gwdb/results/491017863/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:41","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120466R-gwdb","Sample-Other","Water","Groundwater","2014-02-19","08:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490866537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-21",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120466R-gwdb/results/490866537/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:58:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132372-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","13:44:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-46324","YELLOW CAB MW YC-2",{"$nulls":4},32.226975,-110.9677056,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490810236","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132372-gwdb/results/490810236/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:16","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132380-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","08:38:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-57558","YELLOW CAB MW YC-7",{"$nulls":4},32.2274281,-110.9685133,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490899422","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132380-gwdb/results/490899422/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:22:38","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120334R-gwdb","Sample-Other","Water","Groundwater","2014-02-19","07:21:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491006029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-20",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120334R-gwdb/results/491006029/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:11:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120260R-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","10:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490801184","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120260R-gwdb/results/490801184/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:14:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122442-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","08:52:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79222","ADEQ MW-102",{"$nulls":4},32.2461081,-109.8364322,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491018211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-26",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122442-gwdb/results/491018211/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:49","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120422R-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","10:02:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120422R-gwdb/results/490802868/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:37","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120273R-gwdb","Sample-Other","Water","Groundwater","2014-03-20","08:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490939948","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120273R-gwdb/results/490939948/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:15","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121782-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","14:03:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491010114","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121782-gwdb/results/491010114/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:13:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120484R-gwdb","Sample-Other","Water","Groundwater","2014-03-20","07:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490945134","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120484R-gwdb/results/490945134/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:42:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132480-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","10:36:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490899945","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132480-gwdb/results/490899945/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:22:55","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120491R-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","09:20:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769068","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120491R-gwdb/results/490769068/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:47:56","STORET"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302045","Sample-Routine","Water","Surface Water","2013-07-23","09:10:00","EST",{"$nulls":14},"USGS-02350524",null,"L-2060191 Received July 24, 2013  Deleted LC 8252 per Rose.  KB 09/16/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107104896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122410-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","15:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79265","ADEQ MW-105",{"$nulls":4},32.2671364,-109.8474781,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490876852","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122410-gwdb/results/490876852/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:07:04","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122438-gwdb","Sample-Routine","Water","Groundwater","2014-09-25","09:11:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490773971","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122438-gwdb/results/490773971/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:50:12","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120325R-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","08:17:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490768204","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120325R-gwdb/results/490768204/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:47:33","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122424-gwdb","Sample-Routine","Water","Groundwater","2014-09-25","12:07:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490892538","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122424-gwdb/results/490892538/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:18:50","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132475-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","10:25:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490899991","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132475-gwdb/results/490899991/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:22:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122419-gwdb","Sample-Routine","Water","Groundwater","2014-05-20","13:40:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79263","ADEQ MW-103",{"$nulls":4},32.2673994,-109.8469225,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122419-gwdb/results/491017793/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120331R-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","07:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490940182","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120331R-gwdb/results/490940182/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120284R-gwdb","Sample-Routine","Water","Groundwater","2014-05-19","08:17:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-69746","ADEQ MW-10",{"$nulls":4},33.5257597,-112.0815269,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490942859","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120284R-gwdb/results/490942859/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:41:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120415R-gwdb","Sample-Other","Water","Groundwater","2014-02-19","07:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769478","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-21",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120415R-gwdb/results/490769478/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:48:08","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120336R-gwdb","Sample-Routine","Water","Groundwater","2014-03-18","10:18:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65608","ADEQ MW-8",{"$nulls":4},33.5279958,-112.0834425,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490942771","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120336R-gwdb/results/490942771/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:41:32","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122416-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","13:48:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79263","ADEQ MW-103",{"$nulls":4},32.2673994,-109.8469225,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490892459","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122416-gwdb/results/490892459/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:18:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122454-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","07:43:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490892726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122454-gwdb/results/490892726/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:18:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132467-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","10:59:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79228","ADEQ MW-108",{"$nulls":4},32.2459239,-109.8359164,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490811429","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132467-gwdb/results/490811429/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:55","STORET"]
["USGS-MT","USGS Montana Water Science Center","nwismt.01.01301628","Sample-Routine","Water","Surface Water","2013-08-28","10:40:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05014300",null,"L-2410104 Deleted 8252 per Rose.  KB 11/21/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107100098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120286R-gwdb","Sample-Routine","Water","Groundwater","2014-03-19","10:40:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-72800","ADEQ MW-11",{"$nulls":4},33.5244592,-112.0829478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490940480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120286R-gwdb/results/490940480/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132375-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","11:28:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79543","ADEQ MW-4",{"$nulls":4},32.2265778,-110.9674953,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490810186","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-13",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132375-gwdb/results/490810186/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:14","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120423R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:35:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491004827","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120423R-gwdb/results/491004827/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:10:29","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120505R-gwdb","Sample-Routine","Water","Groundwater","2014-03-19","12:52:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79325","ADEQ MW-15",{"$nulls":4},33.5242831,-112.0812317,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490862168","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120505R-gwdb/results/490862168/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:55:36","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120263R-gwdb","Sample-Other","Water","Groundwater","2014-02-19","08:57:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490768108","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-21",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120263R-gwdb/results/490768108/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:47:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132474-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","11:36:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490889957","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132474-gwdb/results/490889957/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:17:23","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120528R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","11:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490947815","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120528R-gwdb/results/490947815/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:43:16","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120499R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:12:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490803083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120499R-gwdb/results/490803083/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122408-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","16:25:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017451","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122408-gwdb/results/491017451/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:27","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122409-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","15:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79263","ADEQ MW-103",{"$nulls":4},32.2673994,-109.8469225,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490880025","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122409-gwdb/results/490880025/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:09:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121779-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","09:48:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490770655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121779-gwdb/results/490770655/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:48:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121777-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","11:46:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491008192","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121777-gwdb/results/491008192/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:12:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120529R-gwdb","Sample-Other","Water","Groundwater","2014-02-19","08:14:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-21",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120529R-gwdb/results/490769537/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:48:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120282R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","09:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490940381","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-01-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120282R-gwdb/results/490940381/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:40:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132473-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","13:38:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490889908","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132473-gwdb/results/490889908/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:17:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122417-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","15:54:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491019357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122417-gwdb/results/491019357/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:18:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122418-gwdb","Sample-Routine","Water","Groundwater","2014-05-20","12:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79264","ADEQ MW-104",{"$nulls":4},32.2674414,-109.8470308,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017719","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122418-gwdb/results/491017719/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:37","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120483R-gwdb","Sample-Other","Water","Groundwater","2014-03-20","07:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491004900","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120483R-gwdb/results/491004900/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:10:32","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122422-gwdb","Sample-Routine","Water","Groundwater","2014-05-20","16:35:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79261","ADEQ MW-101",{"$nulls":4},32.26699,-109.8468803,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490957870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122422-gwdb/results/490957870/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:47:45","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120509R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","11:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490945030","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120509R-gwdb/results/490945030/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:42:16","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120518R-gwdb","Sample-Routine","Water","Groundwater","2014-03-18","14:42:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79326","ADEQ MW-16",{"$nulls":4},33.5245742,-112.0825728,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802738","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120518R-gwdb/results/490802738/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120408R-gwdb","Sample-Routine","Water","Groundwater","2014-03-18","13:42:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79328","ADEQ MW-18",{"$nulls":4},33.5249481,-112.0829158,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490768947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120408R-gwdb/results/490768947/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:47:54","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122432-gwdb","Sample-Routine","Water","Groundwater","2014-09-24","14:49:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490808174","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122432-gwdb/results/490808174/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:19:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122440-gwdb","Sample-Routine","Water","Groundwater","2014-09-24","13:14:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491019476","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122440-gwdb/results/491019476/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:18:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120315R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490801288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120315R-gwdb/results/490801288/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:14:23","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122421-gwdb","Sample-Routine","Water","Groundwater","2014-05-20","14:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79262","ADEQ MW-102",{"$nulls":4},32.26686,-109.8468753,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490808077","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122421-gwdb/results/490808077/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:18:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132379-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","12:45:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79542","ADEQ MW-3A",{"$nulls":4},32.2268128,-110.9672983,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962878","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132379-gwdb/results/490962878/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:47","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122428-gwdb","Sample-Routine","Water","Groundwater","2014-09-25","13:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79226","ADEQ MW-106",{"$nulls":4},32.2460858,-109.8359989,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490880124","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122428-gwdb/results/490880124/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:10:03","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122407-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","16:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79262","ADEQ MW-102",{"$nulls":4},32.26686,-109.8468753,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017375","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122407-gwdb/results/491017375/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:26","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132362-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","15:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-56385","YELLOW CAB MW YC-5",{"$nulls":4},32.2263025,-110.9669419,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490810120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-10",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132362-gwdb/results/490810120/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:12","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120464R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769403","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120464R-gwdb/results/490769403/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:48:06","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120299R-gwdb","Sample-Routine","Water","Groundwater","2014-03-19","11:20:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-72801","ADEQ MW-12",{"$nulls":4},33.5246214,-112.0828678,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490768568","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120299R-gwdb/results/490768568/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:47:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122455-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","08:12:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490895029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122455-gwdb/results/490895029/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:19:59","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132374-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","17:25:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-57556","YELLOW CAB RW-1",{"$nulls":4},32.2267939,-110.9675289,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490963014","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132374-gwdb/results/490963014/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:49","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132466-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","13:58:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79224","ADEQ MW-104",{"$nulls":4},32.2460894,-109.8361219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490811282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-18",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132466-gwdb/results/490811282/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:20:52","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120310R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","09:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802143","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-01-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120310R-gwdb/results/490802143/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120311R-gwdb","Sample-Other","Water","Groundwater","2014-03-20","06:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491006094","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120311R-gwdb/results/491006094/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:11:23","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120456R-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","09:31:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490865893","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120456R-gwdb/results/490865893/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:58:02","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132366-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","11:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-46324","YELLOW CAB MW YC-2",{"$nulls":4},32.226975,-110.9677056,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490961619","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132366-gwdb/results/490961619/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132370-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","10:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-57558","YELLOW CAB MW YC-7",{"$nulls":4},32.2274281,-110.9685133,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490899332","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132370-gwdb/results/490899332/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:22:35","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132369-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","12:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-57557","YELLOW CAB MW YC-6",{"$nulls":4},32.2262906,-110.968795,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490883064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-10",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132369-gwdb/results/490883064/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:12:58","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120326R-gwdb","Sample-Other","Water","Groundwater","2014-02-19","07:40:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490942497","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-21",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120326R-gwdb/results/490942497/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:41:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120498R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","11:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79323","ADEQ MW-3R",{"$nulls":4},33.5244781,-112.0817017,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491004706","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120498R-gwdb/results/491004706/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:10:26","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122443-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","07:58:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490808223","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122443-gwdb/results/490808223/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:19:01","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120482R-gwdb","Sample-Other","Water","Groundwater","2014-02-19","08:20:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490866448","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-21",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120482R-gwdb/results/490866448/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:58:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122439-gwdb","Sample-Routine","Water","Groundwater","2014-09-25","11:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017894","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122439-gwdb/results/491017894/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122456-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","08:28:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491018104","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122456-gwdb/results/491018104/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:17:46","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132468-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","14:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79226","ADEQ MW-106",{"$nulls":4},32.2460858,-109.8359989,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490964831","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132468-gwdb/results/490964831/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:50:32","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122445-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","07:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490877099","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122445-gwdb/results/490877099/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:07:17","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120409D-gwdb","Quality Control Sample-Field Replicate","Water","Groundwater","2014-03-18","12:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79327","ADEQ MW-17",{"$nulls":4},33.5244989,-112.0835889,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802805","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120409D-gwdb/results/490802805/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:33","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122430-gwdb","Sample-Routine","Water","Groundwater","2014-09-24","12:37:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490892640","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122430-gwdb/results/490892640/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:18:54","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132367-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","11:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79542","ADEQ MW-3A",{"$nulls":4},32.2268128,-110.9672983,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882914","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132367-gwdb/results/490882914/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:12:50","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120349R-gwdb","Sample-Routine","Water","Groundwater","2014-03-18","11:36:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65606","ADEQ MW-6",{"$nulls":4},33.5257544,-112.0803806,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490865382","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120349R-gwdb/results/490865382/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:57:44","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132378-gwdb","Sample-Routine","Water","Groundwater","2014-06-04","18:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-56385","YELLOW CAB MW YC-5",{"$nulls":4},32.2263025,-110.9669419,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490776066","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132378-gwdb/results/490776066/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:51:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120480R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:08:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491004764","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120480R-gwdb/results/491004764/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:10:27","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120463R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","11:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769361","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120463R-gwdb/results/490769361/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:48:05","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132365-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","11:40:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79541","ADEQ MW-1A",{"$nulls":4},32.2267986,-110.967605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490961492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132365-gwdb/results/490961492/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:49:26","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120262R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-62913","ADEQ MW-3",{"$nulls":4},33.52445,-112.0817389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490861459","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120262R-gwdb/results/490861459/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:55:04","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120285R-gwdb","Sample-Routine","Water","Groundwater","2014-03-19","07:12:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-69747","ADEQ MW-09",{"$nulls":4},33.5248189,-112.0815725,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491001718","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120285R-gwdb/results/491001718/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:08:53","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122411-gwdb","Sample-Routine","Water","Groundwater","2014-03-20","15:20:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79264","ADEQ MW-104",{"$nulls":4},32.2674414,-109.8470308,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490960165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122411-gwdb/results/490960165/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:48:55","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121781-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","06:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79325","ADEQ MW-15",{"$nulls":4},33.5242831,-112.0812317,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490946186","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121781-gwdb/results/490946186/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:42:37","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122414-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","14:48:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79262","ADEQ MW-102",{"$nulls":4},32.26686,-109.8468753,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490957723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122414-gwdb/results/490957723/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:47:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122433-gwdb","Sample-Routine","Water","Groundwater","2014-09-25","08:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490773898","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122433-gwdb/results/490773898/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T16:50:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120317R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","10:35:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490859565","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-01-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120317R-gwdb/results/490859565/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:54:03","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120316R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","10:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490801694","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-01-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120316R-gwdb/results/490801694/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:14:46","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120476R-gwdb","Sample-Routine","Water","Groundwater","2014-03-18","15:32:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79327","ADEQ MW-17",{"$nulls":4},33.5244989,-112.0835889,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491006542","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120476R-gwdb/results/491006542/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:11:42","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132364-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","10:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79544","ADEQ MW-9",{"$nulls":4},32.2270219,-110.9675036,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490897231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132364-gwdb/results/490897231/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:21:08","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120446R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","11:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79324","ADEQ MW-14",{"$nulls":4},33.5246394,-112.0816944,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490944937","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120446R-gwdb/results/490944937/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T18:42:14","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120266D-gwdb","Quality Control Sample-Field Replicate","Water","Groundwater","2014-03-20","12:00:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491001655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120266D-gwdb/results/491001655/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T19:08:50","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120481R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","12:17:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490803205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-02-01",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120481R-gwdb/results/490803205/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2015-11-30T17:15:49","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148945-gwdb","Sample-Other","Water","Groundwater","2015-10-22","16:04:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65186","MW-203M",{"$nulls":4},33.4799944,-112.1385917,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552065549","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148945-gwdb/results/552065549/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:28:45","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147106-gwdb","Sample-Routine","Water","Groundwater","2015-01-05","17:55:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80123","ADEQ MW-3R",{"$nulls":4},33.4317064,-112.0749236,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551974298","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-01-10",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147106-gwdb/results/551974298/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:30:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148936-gwdb","Sample-Other","Water","Groundwater","2015-10-22","14:18:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-70420","ADEQ MW-208S",{"$nulls":4},33.4665278,-112.1618058,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552096284","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148936-gwdb/results/552096284/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:41:07","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147216-gwdb","Sample-Routine","Water","Groundwater","2015-08-18","09:35:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79862","ADEQ MW-2",{"$nulls":4},33.9350089,-114.0081389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551974662","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-08-26",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147216-gwdb/results/551974662/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:31:04","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144192-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","09:59:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552132509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144192-gwdb/results/552132509/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:57:17","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147003-gwdb","Sample-Routine","Water","Groundwater","2015-05-28","16:20:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79868","ADEQ MW-8",{"$nulls":4},33.935015,-114.008115,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552031283","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147003-gwdb/results/552031283/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:10:27","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148337-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","10:14:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551977753","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148337-gwdb/results/551977753/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:32:53","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148941-gwdb","Sample-Other","Water","Groundwater","2015-10-23","12:42:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65188","MW-205S",{"$nulls":4},33.4826306,-112.1361583,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552139857","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148941-gwdb/results/552139857/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:00:54","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148970-gwdb","Sample-Routine","Water","Groundwater","2015-11-19","17:53:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552175277","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148970-gwdb/results/552175277/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:15:45","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148969-gwdb","Sample-Routine","Water","Groundwater","2015-11-20","10:48:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79226","ADEQ MW-106",{"$nulls":4},32.2460858,-109.8359989,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551995975","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148969-gwdb/results/551995975/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:48:22","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147217-gwdb","Sample-Routine","Water","Groundwater","2015-08-18","07:00:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79868","ADEQ MW-8",{"$nulls":4},33.935015,-114.008115,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552126858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-08-26",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147217-gwdb/results/552126858/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:54:47","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148929-gwdb","Sample-Other","Water","Groundwater","2015-10-23","14:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-60383","WCP-204",{"$nulls":4},33.4819272,-112.1311575,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551993247","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148929-gwdb/results/551993247/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:47:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144188-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","10:19:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552132539","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144188-gwdb/results/552132539/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:57:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147107-gwdb","Sample-Routine","Water","Groundwater","2015-01-05","19:15:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80121","ADEQ MW-1R",{"$nulls":4},33.4316522,-112.0748403,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552082684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-01-10",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147107-gwdb/results/552082684/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:37:47","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147212-gwdb","Sample-Routine","Water","Groundwater","2015-08-18","13:30:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79861","ADEQ MW-1",{"$nulls":4},33.9350956,-114.0081756,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552162080","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-08-26",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147212-gwdb/results/552162080/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:12:12","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148334-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","09:58:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552170447","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148334-gwdb/results/552170447/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:14:17","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148982-gwdb","Sample-Routine","Water","Groundwater","2015-11-19","12:52:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552037405","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148982-gwdb/results/552037405/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:14:22","STORET"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01300594","Sample-Routine","Water","Surface Water","2013-06-18","12:10:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-13210360",null,"L-1710091 ID user code per Romanok, paa, 6/20/13  Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107112487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147110-gwdb","Sample-Routine","Water","Groundwater","2015-03-22","12:25:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80121","ADEQ MW-1R",{"$nulls":4},33.4316522,-112.0748403,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552051371","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-03-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147110-gwdb/results/552051371/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:22:46","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144194-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","10:36:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79231","ADEQ MW-111",{"$nulls":4},32.2457594,-109.8359936,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552085057","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144194-gwdb/results/552085057/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:38:26","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148341-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","13:49:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79223","ADEQ MW-103",{"$nulls":4},32.2459961,-109.8361039,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551992642","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148341-gwdb/results/551992642/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:47:06","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148951-gwdb","Sample-Other","Water","Groundwater","2015-10-22","12:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65029","MW-110M",{"$nulls":4},33.4856661,-112.1612975,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552139610","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148951-gwdb/results/552139610/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:00:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146998-gwdb","Sample-Routine","Water","Groundwater","2015-05-28","12:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79869","ADEQ MW-9",{"$nulls":4},33.9350128,-114.0081956,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552158519","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146998-gwdb/results/552158519/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:11:13","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148978-gwdb","Sample-Routine","Water","Groundwater","2015-11-20","11:48:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79224","ADEQ MW-104",{"$nulls":4},32.2460894,-109.8361219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551995908","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148978-gwdb/results/551995908/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:48:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150558-gwdb","Sample-Routine","Water","Groundwater","2015-09-24","10:00:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80595","MW-4",{"$nulls":4},33.4930494,-113.16208,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552016236","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150558-gwdb/results/552016236/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:00:57","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144187-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","10:11:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552084998","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144187-gwdb/results/552084998/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:38:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148928-gwdb","Sample-Other","Water","Groundwater","2015-10-23","12:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-58082","WOC MW-201S",{"$nulls":4},33.4803331,-112.136605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551979065","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148928-gwdb/results/551979065/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:34:13","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144189-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","11:07:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552006944","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144189-gwdb/results/552006944/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:55:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148972-gwdb","Sample-Routine","Water","Groundwater","2015-11-20","08:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552140069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148972-gwdb/results/552140069/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:01:03","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144202-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","11:36:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552006996","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144202-gwdb/results/552006996/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:55:50","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147019-gwdb","Sample-Routine","Water","Groundwater","2015-06-26","09:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552109524","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-07-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147019-gwdb/results/552109524/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:49:52","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147012-gwdb","Sample-Routine","Water","Groundwater","2015-06-26","12:45:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79231","ADEQ MW-111",{"$nulls":4},32.2457594,-109.8359936,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552156018","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-07-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147012-gwdb/results/552156018/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:10:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148332-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","12:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79223","ADEQ MW-103",{"$nulls":4},32.2459961,-109.8361039,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551977852","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-06",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148332-gwdb/results/551977852/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:32:55","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144450-gwdb","Sample-Routine","Water","Groundwater","2015-02-26","14:08:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79861","ADEQ MW-1",{"$nulls":4},33.9350956,-114.0081756,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552010038","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-03-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144450-gwdb/results/552010038/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:58:47","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148342-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","11:34:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552061482","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148342-gwdb/results/552061482/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:26:53","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147001-gwdb","Sample-Routine","Water","Groundwater","2015-05-28","09:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79868","ADEQ MW-8",{"$nulls":4},33.935015,-114.008115,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551966687","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147001-gwdb/results/551966687/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:23:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148329-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","12:59:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79226","ADEQ MW-106",{"$nulls":4},32.2460858,-109.8359989,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552135625","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148329-gwdb/results/552135625/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:58:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147000-gwdb","Sample-Routine","Water","Groundwater","2015-05-28","11:20:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79862","ADEQ MW-2",{"$nulls":4},33.9350089,-114.0081389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552158472","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-06-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147000-gwdb/results/552158472/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:11:12","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144186-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","12:25:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79224","ADEQ MW-104",{"$nulls":4},32.2460894,-109.8361219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552132723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144186-gwdb/results/552132723/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:57:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148934-gwdb","Sample-Other","Water","Groundwater","2015-10-22","10:44:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-70418","ADEQ MW-3SR",{"$nulls":4},33.4897036,-112.1385081,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551978904","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148934-gwdb/results/551978904/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:34:02","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144193-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","10:27:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79233","ADEQ MW-113",{"$nulls":4},32.2460908,-109.8357894,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552131257","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144193-gwdb/results/552131257/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:56:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150571-gwdb","Sample-Routine","Water","Groundwater","2015-09-24","14:57:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80596","MW-5",{"$nulls":4},33.4929703,-113.1628769,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552089940","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150571-gwdb/results/552089940/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:39:35","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148980-gwdb","Sample-Routine","Water","Groundwater","2015-11-19","16:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79231","ADEQ MW-111",{"$nulls":4},32.2457594,-109.8359936,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552096478","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148980-gwdb/results/552096478/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:41:12","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147017-gwdb","Sample-Routine","Water","Groundwater","2015-06-26","13:20:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79230","ADEQ MW-110",{"$nulls":4},32.2459061,-109.8364183,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552155938","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-07-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147017-gwdb/results/552155938/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:10:32","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147214-gwdb","Sample-Routine","Water","Groundwater","2015-08-18","11:30:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79863","ADEQ MW-3",{"$nulls":4},33.9349981,-114.0080689,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551974750","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-08-26",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147214-gwdb/results/551974750/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:31:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147014-gwdb","Sample-Routine","Water","Groundwater","2015-06-26","15:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79222","ADEQ MW-102",{"$nulls":4},32.2461081,-109.8364322,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552109464","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-07-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147014-gwdb/results/552109464/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:49:51","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144453-gwdb","Sample-Routine","Water","Groundwater","2015-02-26","08:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79868","ADEQ MW-8",{"$nulls":4},33.935015,-114.008115,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551968716","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-03-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144453-gwdb/results/551968716/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:27:24","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148948-gwdb","Sample-Other","Water","Groundwater","2015-10-22","12:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64631","MW-105M",{"$nulls":4},33.4868192,-112.1441442,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552169128","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148948-gwdb/results/552169128/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:13:52","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147016-gwdb","Sample-Routine","Water","Groundwater","2015-06-26","14:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551974029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-07-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147016-gwdb/results/551974029/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:30:23","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148327-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","11:06:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79231","ADEQ MW-111",{"$nulls":4},32.2457594,-109.8359936,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552061561","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148327-gwdb/results/552061561/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:26:55","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148330-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","12:02:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79227","ADEQ MW-107",{"$nulls":4},32.2464336,-109.8361044,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551992681","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148330-gwdb/results/551992681/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:47:07","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144198-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","11:24:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552159494","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144198-gwdb/results/552159494/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:11:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150574-gwdb","Sample-Routine","Water","Groundwater","2015-09-24","11:10:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80593","MW-2",{"$nulls":4},33.4927864,-113.1616206,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552130594","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150574-gwdb/results/552130594/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:56:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148338-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","12:16:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552061423","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148338-gwdb/results/552061423/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:26:51","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144449-gwdb","Sample-Routine","Water","Groundwater","2015-02-26","11:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79869","ADEQ MW-9",{"$nulls":4},33.9350128,-114.0081956,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551968642","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-03-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144449-gwdb/results/551968642/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T01:27:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144201-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","10:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79228","ADEQ MW-108",{"$nulls":4},32.2459239,-109.8359164,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552159435","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144201-gwdb/results/552159435/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:11:27","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148946-gwdb","Sample-Other","Water","Groundwater","2015-10-22","09:50:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57155","WOC MW-04M",{"$nulls":4},33.4891086,-112.1367756,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552096171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148946-gwdb/results/552096171/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:41:03","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147022-gwdb","Sample-Routine","Water","Groundwater","2015-06-26","16:50:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79224","ADEQ MW-104",{"$nulls":4},32.2460894,-109.8361219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552101718","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-07-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147022-gwdb/results/552101718/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:44:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148938-gwdb","Sample-Other","Water","Groundwater","2015-10-22","11:06:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57150","WOC MW-02M",{"$nulls":4},33.4879081,-112.1384033,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552171245","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148938-gwdb/results/552171245/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:14:33","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148952-gwdb","Sample-Other","Water","Groundwater","2015-10-22","13:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65027","WOC-108M",{"$nulls":4},33.4810242,-112.1675131,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552065403","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148952-gwdb/results/552065403/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:28:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150570-gwdb","Sample-Routine","Water","Groundwater","2015-09-24","14:12:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80595","MW-4",{"$nulls":4},33.4930494,-113.16208,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552133022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150570-gwdb/results/552133022/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T02:57:26","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148979-gwdb","Sample-Routine","Water","Groundwater","2015-11-20","08:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552175226","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148979-gwdb/results/552175226/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:15:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148975-gwdb","Sample-Routine","Water","Groundwater","2015-11-19","12:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79235","ADEQ MW-115",{"$nulls":4},32.2457614,-109.8356147,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552175408","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148975-gwdb/results/552175408/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:15:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-151691.CHEM","Sample-Routine","Water","Groundwater","2016-03-16","09:58:00","EST",{"$nulls":4},155,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-55159",67697,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.4719174,-112.1439212,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-799539067","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-03-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-151691.CHEM/results/799539067/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2019-10-07T11:07:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-151701-gwdb","Sample-Other","Water","Groundwater","2016-03-16","11:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65029","MW-110M",{"$nulls":4},33.4856661,-112.1612975,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552147608","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-151701-gwdb/results/552147608/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",null,"2016-05-12T03:07:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25043.CHEM","Sample-Routine","Water","Groundwater","2020-01-21","11:24:00","MST",{"$nulls":4},9.46,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","WESTERN TECHNOLOGY INC.","AZDEQ_WPD-61719",81426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0354222,-110.7224972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-829102069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,9.46,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25043.CHEM/results/829102069/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2020-03-18T11:28:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28852.CHEM","Sample-Routine","Other","Groundwater","2019-10-03","12:54:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856014543","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28852.CHEM/results/856014543/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2020-09-10T09:53:45","STORET"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400284","Sample-Routine","Water","Surface Water","2014-04-15","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214655255",null,"A-1070012 10 min time offset",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97702315","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400378","Sample-Routine","Water","Surface Water","2014-04-16","10:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0208524090",null,"A-1070135 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97747492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401154","Sample-Routine","Water","Surface Water","2014-06-11","13:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02095181",null,"L-1690057 Received June17, 2014",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98459973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401199","Sample-Routine","Water","Surface Water","2014-06-11","16:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0212430653",null,"L-1690092 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98477301","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401205","Sample-Routine","Water","Surface Water","2014-06-11","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0212467595",null,"A-1680169 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98478357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44371.CHEM","Sample-Routine","Other","Groundwater","2023-02-09","01:54:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992961989","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44371.CHEM/results/992961989/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:43:06","STORET"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400735","Sample-Routine","Water","Surface Water","2014-05-13","10:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02085500",null,"L-1360081 Received May 15, 2014..  ASR date changed from 20140512 to 20140513 per Cassy P,paa,6/6/14",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97955558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46585.CHEM","Sample-Routine","Other","Groundwater","2023-05-09","01:32:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992982912","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46585.CHEM/results/992982912/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:45:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50992.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","04:09:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035741","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50992.CHEM/results/993035741/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50994.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","02:13:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035877","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50994.CHEM/results/993035877/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51530.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:57:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63544",82855,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258612,-110.9668172,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038906","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51530.CHEM/results/993038906/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52420.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:59:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361846","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52420.CHEM/results/997361846/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:47","STORET"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401189","Sample-Routine","Water","Surface Water","2014-06-10","14:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214265808",null,"L-1690115 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98465895","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52424.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:01:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362118","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52424.CHEM/results/997362118/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",null,"2023-12-29T09:53:48","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-151696-gwdb","Sample-Other","Water","Groundwater","2016-03-16","12:12:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57159","WOC MW-06M",{"$nulls":4},33.4839803,-112.1425672,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552028687","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-151696-gwdb/results/552028687/resdetectqntlmts","Lower Reporting Limit",0.01,"mg/L",null,"2016-05-12T02:08:11","STORET"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01402046","Sample-Routine","Water","Surface Water","2014-06-11","09:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02207435",null,"A-1680209 4 Drops HCl",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98396156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29068.CHEM","Sample-Routine","Other","Groundwater","2019-12-12","11:43:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909406","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29068.CHEM/results/859909406/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",null,"2020-10-14T17:37:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29071.CHEM","Sample-Routine","Other","Groundwater","2019-12-11","10:18:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909601","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29071.CHEM/results/859909601/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",null,"2020-10-14T17:37:39","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132476-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","14:32:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79223","ADEQ MW-103",{"$nulls":4},32.2459961,-109.8361039,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490811206","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132476-gwdb/results/490811206/resdetectqntlmts","Lower Reporting Limit",0.05,"mg/L",null,"2015-11-30T17:20:50","STORET"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300200","Sample-Routine","Water","Groundwater","2013-08-13","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333036081442108",null,"L-2270106 Received August 14, 2013  LC1792 corrected to Scgedule 1792, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1100..  time added to ASR per radon, paa, 8/15/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95650577","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300810","Sample-Routine","Water","Groundwater","2013-08-26","13:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382403075233201",null,"L-2400035 Received August 27, 2013",null,"Not applicable","Routine sample",null,null,4044,"USGS parameter code 82398","Submersible jet pump",null,"Submersible positive-pressure pump","NWIS-96270095","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301280","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303501087174801",null,"L-2610137 Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96718520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400292","Sample-Routine","Water","Groundwater","2013-12-03","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500119590001",null,"L-3380016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01401641","Sample-Routine","Water","Surface Water","2014-05-16","08:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02336120",null,"A-1400253 2002943  10 min offset",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97962970","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300111","Sample-Routine","Water","Groundwater","2013-08-05","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311928085494201",null,"L-2180068 Samples were received chilled at the WHOI lab.","Tallahatta Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96823327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400243","Sample-Routine","Water","Groundwater","2013-11-20","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370200120280001",null,"L-3290106 X=a PEST is a PEST, not a GCV    Received November 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775206","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301260","Sample-Routine","Water","Groundwater","2013-09-24","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362244077015501",null,"L-2690096 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96580695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301225","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351119076404801",null,"L-2630111 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110389902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305612","Sample-Routine","Water","Groundwater","2013-07-25","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364457119553501",null,"L-2100109 S2437 PEST split to separate ASR @1331, paa, 7/29/13    Received July 26, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95227473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01401179","Sample-Routine","Water","Surface Water","2014-04-17","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02336410",null,"A-1120107 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97680305","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301269","Sample-Routine","Water","Groundwater","2013-09-24","16:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351731076514101",null,"L-2700088 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110393177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306534","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420001",null,"L-2610074 Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96538536","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300316","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354709115220001",null,"L-2680157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96730762","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401183","Sample-Routine","Water","Surface Water","2014-06-11","08:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02146470",null,"L-1690040 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98464836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301071","Sample-Routine","Water","Groundwater","2013-09-03","16:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344734077254601",null,"L-2490159 Radon recvd completely unlabeled, added label per ASR, WSC notified requesting verify, paa, 9/4/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96378578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300704","Sample-Routine","Water","Groundwater","2013-07-23","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-374755075371001",null,"L-2060179 Received July 24, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95055836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300348","Sample-Routine","Water","Groundwater","2013-08-19","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313610091504501",null,"L-2320151 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95555138","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302165","Sample-Routine","Water","Groundwater","2013-08-13","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312346084520401",null,"L-2270074 Received August 14, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96562393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300298","Sample-Routine","Water","Groundwater","2013-09-11","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405030115500001",null,"L-2550083 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573942","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400018","Sample-Routine","Water","Groundwater","2013-10-28","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",477,"feet",538,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375541076514301",null,"L-3030063 Received October 29, 2013  Samples were received chilled at the WHOI lab.  sta id corrected to 4301 per A. Melberg, paa, 1/21/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96781964","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302198","Sample-Routine","Water","Groundwater","2013-09-24","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320348084132701",null,"L-2680108 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96632220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300477","Sample-Routine","Water","Groundwater","2013-09-11","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304921092402202",null,"L-2550097 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96471207","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302913","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-275725097562701",null,"L-2550106 ASRs recvd late & entered 1/21/14, paa  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96453689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300941","Sample-Routine","Water","Groundwater","2013-08-13","15:00:00","EDT",{"$nulls":6},"Below land-surface datum",52,"feet",67,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-394208082252201",null,"L-2270196 Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96559417","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301268","Sample-Routine","Water","Groundwater","2013-09-24","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350420077084901",null,"L-2700188 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110392721","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300317","Sample-Routine","Water","Groundwater","2013-09-23","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361023115114401",null,"L-2670013 ASR time 0900 (corrected from 9000), paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96731214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300275","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302832090064101",null,"L-2210134 WHOI ASR missing alkalinity, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95430725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300202","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335128081250001",null,"L-2340223 Samples were received chilled at the WHOI lab.  Sch 1792 not LC1792, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95651065","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400087","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-20","11:00:00","CST",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-443306094125501",null,"L-3250095 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96957832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300101","Sample-Routine","Water","Groundwater","2013-08-06","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361045082225501",null,"A-2200033 2 drops of HCL added to VOCs  Actual Radon Time: 14:55 EDT L-2200033 Received August 7, 2013  WHOI ASR missing pH & alk, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95427218","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300418","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321642111143301",null,"L-2210123 Received August 08, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-97270325","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300157","Sample-Routine","Water","Groundwater","2013-07-10","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325116087570601",null,"L-1920079 X = No Station ID on samples..  S2437 split to 20131920166, paa, 2/19/14  Samples were received chilled at the WHOI lab.  X = Station ID not on label","Gordo Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97167992","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500568","Sample-Routine","Water","Surface Water","2015-06-22","13:30:00","CST",{"$nulls":13},"USGS - Illinois Water Science Center","USGS-05537000",null,"A-1770033 Attn: Mississippi River Study.",null,"Rising stage","Routine sample",null,null,15,"USGS parameter code 82398","10 or more equal width verticals, equal non-iso transit rate limited by velocity",null,"Weighted-bottle sampler","NWIS-101100449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305900","Sample-Routine","Water","Groundwater","2013-08-13","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372502",null,"L-2260085 FA btl condition changed to improper preservation, JNV   Lab acidification lab code 3105 added, JNV   FA preserved by C.Harris on 8/15/13 @ 10:00, JNV  ASR missing field alk values for WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95532138","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300566","Sample-Routine","Water","Groundwater","2013-06-06","11:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-385208075460801",null,"L-1620022 Received June 07, 2013..  S2437 split to 20131620255, paa, 2/14/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94535410","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500975","Sample-Routine","Water","Surface Water","2015-08-26","13:00:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05543500",{"$nulls":3},"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-101745018","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500413","Sample-Routine","Water","Surface Water","2015-05-07","10:30:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05541510",null,"L-1320087 X=no btl types on GCC, GCV, OXW, PEST, PHARM and TOC, no schedule or lab codes on btls   Received May 09, 2015..  Emailed WSC contact, missing proposal # for LC 9030,3406,9031,4440, & 8099, ACW, 5/13/15 Added proposal # CL15023, ACW, 5/19/15",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-100743136","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-14","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404279","Sample-Routine","Water","Groundwater","2014-08-12","12:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-360000120540001",null,"L-2250105 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-105559145","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01401004","Sample-Routine","Water","Groundwater","2014-08-21","09:00:00","EST",{"$nulls":6},"Below land-surface datum",null,null,164,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385521078281601",null,"L-2370020 Received August 22, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99097093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01401011","Sample-Routine","Water","Groundwater","2014-02-04","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363325119440901",null,"L-0360010 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106781269","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-02-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402129","Sample-Routine","Water","Groundwater","2014-07-08","11:00:00","CST",{"$nulls":4},350,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-425837090375701",null,"L-1900079 S1792 changed to S1979 by TAL, paa","Ordovician-Cambrian Systems","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-113355283","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402934","Sample-Routine","Water","Groundwater","2014-05-15","11:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-383703121280701",null,"L-1360122 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112107161","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-30","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01401667","Sample-Routine","Water","Groundwater","2014-05-20","10:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314749106210801",null,"L-1410115 Updated SID from 314751106220501 per Ging.  KB 8/28/14  ASR missing mandatory pH & alk, paa   Fields added per Ging, paa, 6/3/14 Samples were received chilled at the WHOI lab.      per Ging corrected station id  pwg  10/17/14  per Ging corrected station id  pwg  10/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99164626","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402173","Sample-Routine","Water","Groundwater","2014-07-10","10:00:00","CST",{"$nulls":4},90,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-433144089595901",null,"A-1920111 Alternate contact-Kelly Warner (klwarner)/217-328-09727 PR14205:Split Sample  (alternate contact-Kelly Warner, klwarner@usgs.gov, 217-328-9725). Acidified with HNO3. RADCHEM-acidified HNO  Actual Radon Time = 0910 CDT Separate FedEx Box  Alternate contact - Kelly Warner (klwarner) 217-328-","Ordovician-Cambrian Systems","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-113356499","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404089","Sample-Routine","Water","Groundwater","2014-08-05","10:50:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500121470001",null,"L-2230024 Received August 08, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-106884472","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400984","Sample-Routine","Water","Groundwater","2014-01-29","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364600119540001",null,"L-0310049 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-106779826","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-02-11","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01401000","Sample-Routine","Water","Groundwater","2014-08-20","10:00:00","EST",{"$nulls":6},"Below land-surface datum",62,"feet",605,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384600078383801",null,"L-2340027 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99096176","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01400857","Sample-Routine","Water","Groundwater","2014-07-24","09:55:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-475003098313701",null,"L-2090183 Received July 25, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-98828242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01500422","Sample-Routine","Water","Groundwater","2014-12-04","09:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361100119010001",null,"L-3390078 7th GCV is actually a PHARM,paa,12/5/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104659895","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-12-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MT","USGS Montana Water Science Center","nwismt.01.01400468","Sample-Routine","Water","Groundwater","2014-04-10","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-474050114084801",null,"L-1010127 Samples were received chilled at the WHOI lab.","Drift","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97712432","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01402574","Sample-Routine","Water","Groundwater","2014-08-07","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335137082444801",null,"L-2200210 X=improper sample container=DOC- Green Cap  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-98875666","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01400576","Sample-Routine","Water","Groundwater","2014-06-03","09:00:00","CDT",{"$nulls":6},"Below land-surface datum",404,"feet",424,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345352090044301",null,"L-1550149 FUS btl tye, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-98603668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01400645","Sample-Routine","Water","Groundwater","2014-07-02","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",700,"feet",800,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324806090553601",null,"L-1880024 Received July 03, 2014  FUS btl type, not GCC, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-98722651","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01400594","Sample-Routine","Water","Groundwater","2014-06-05","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",71,"feet",96,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342155089305401",null,"L-1570270 X=please dont use pencil on ASR  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-98615855","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400766","Sample-Routine","Water","Groundwater","2014-01-07","12:50:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-362100119520001",null,"L-0100028 S1792 (LC2802) deleted and LC3107/3108 added per TAL and Mullin, paa, 3/6/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106778223","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-01-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404630","Sample-Routine","Water","Groundwater","2014-09-15","11:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-383916122473501",null,"L-2610121 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106888016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01400964","Sample-Routine","Water","Groundwater","2014-08-11","11:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394004076045301",null,"L-2240155 Schedule 2440 entered per ASR comment, ASR does not support seven schedules, paa, 8/13/14  Samples were received chilled at the WHOI lab.  Schedule 1792 not LC1792, paa corrected, 8/20/14","Marburg Formation","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99049021","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01401830","Sample-Routine","Water","Groundwater","2014-07-16","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","MN040-443143093544601",null,"L-1990089 X=time on bottles is 1100, date on bottles is 7/16/14added date and time to ASR and LIM's   pwg  Added agency code per Langer.  KB 9/4/14  Date & time added to ASR by TAL & per btls, paa  X=no date or time on sample    added date and time to ASR and data base per Michael M.  pwg  7/18/14",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-98724340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402569","Sample-Routine","Water","Groundwater","2014-04-22","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-331710116415401",null,"L-1190090 Received April 26, 2014 Chilled containers received warm at 7.6   Degrees C..  recvd warm 3/26, ok log per Dugan, PG  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-112105051","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-01","sample was warm when receivedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404830","Sample-Routine","Water","Groundwater","2014-09-24","10:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420003",null,"L-2680032 S2755 added per Mathany,S1306 deleted and S4443 added per Justin K,paa,9/25/14..  S4443 deleted per Mathany/Rose, paa, 9/30/14  Samples were received chilled at the WHOI lab.  X=improper sample container - sample sent in 40mL btl..  proposal corrected to CL14NAWCA per Mathany, paa, 12/8/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99371220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01402426","Sample-Routine","Water","Groundwater","2014-07-17","10:30:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353443106191301",null,"L-2020114 Received July 18, 2014  S1792 not LC, paa  Samples were received chilled at the WHOI lab.  X=improper sample container for HFL =250",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109719881","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01400483","Sample-Routine","Water","Groundwater","2014-04-02","11:30:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-422855093481501",null,"L-0930033 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-97579983","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400584","Sample-Routine","Water","Groundwater","2014-06-25","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","MN040-450247092502201",null,"A-1770154 VOCs HAVE 5 DROPS HCL EACH VIAL   Please Lab Filter Schedule 2434  PR14205: Split Sample  GW-RADCHEM-- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH2  PR14205:Split sample  RADON SAMPLE (Mailed in Fed-Ex Box) alone  Exact Time: 10:35  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-98559845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01403458","Sample-Routine","Water","Groundwater","2014-08-26","11:00:00","CST",{"$nulls":6},"Below land-surface datum",170,"feet",null,null,"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-440203089311001",null,"L-2400070 Received August 27, 2014  Samples were received chilled at the WHOI lab.","Ordovician-Cambrian Systems","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-113392941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01601254","Sample-Routine","Water","Groundwater","2015-12-07","14:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-293516098325501",null,"L-3420044 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible helical rotor pump","NWIS-103125822","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-11","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01501719","Quality Control Sample-Field Replicate","Water","Groundwater","2015-01-13","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361700119340001",null,"L-0140025 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112108390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-01-23","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01500328","Sample-Routine","Water","Groundwater","2015-04-21","08:18:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-433334112565501",null,"L-1130147 S1380 deleted and S4436 added per Maimer,D. Rose verified,paa,4/27/15",null,"Not determined","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-100500334","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-29","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01501789","Sample-Routine","Water","Groundwater","2015-06-09","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-310224083113001",null,"L-1638710 Samples were received chilled at the WHOI lab.    Changed station ID to 310224083113001 perC. Younker, ACW, 9/21/15",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-101187609","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-12","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01501435","Sample-Routine","Water","Groundwater","2015-05-13","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-383455101454001",null,"L-1340077 X=no station ids on PEST or PHARM btls  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,8040,"USGS parameter code 82398","Spigot",null,"Jet pump","NWIS-100823925","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-16","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01502277","Sample-Routine","Water","Groundwater","2015-02-25","12:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361200119420001",null,"L-0580068 FED EX LATE DELIVERY  Sulfide odor detected Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104663339","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-02-28","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01502641","Sample-Routine","Water","Groundwater","2015-03-18","13:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-360700119150001",null,"L-0790091 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104664958","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-03-28","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01600117","Sample-Routine","Water","Groundwater","2015-10-05","11:28:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-433315112560301",null,"A-2800030 Please sign and return chain of custody form.",null,"Not applicable","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-102038121","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-10-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600449","Sample-Routine","Water","Groundwater","2015-12-02","12:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364355119484601",null,"L-3380086 X=no sta id, date or time on GCV's",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106939129","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-08","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01501803","Sample-Routine","Water","Groundwater","2015-06-11","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-313242082291601",null,"L-1630092 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-101190109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-16","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600559","Sample-Routine","Water","Groundwater","2015-12-08","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391300120590001",null,"A-3430037 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112116437","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-11","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500792","Sample-Routine","Water","Groundwater","2015-04-23","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-264460080406001",null,"L-1170058 Received April 24, 2015  1792 switched to 1979 due to high solids  H2S =Yes 76ug/L Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-109652028","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500785","Sample-Routine","Water","Groundwater","2015-08-11","10:00:00","CDT",{"$nulls":4},14.5,"feet",null,15.9,"feet",20.9,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-384629090350901",null,"A-2240122 Alternate contact-Kelly Warner(klwarner)/217-328-09727   drops HCL for VOC  Alternate contact - Kelly Warner,klwarner@usgs.gov 217-328-9725. Acidified with HNO3. Acidified with HNO3. RADCHEM - acidified HNO3","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101522133","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-15","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600112","Sample-Routine","Water","Groundwater","2015-10-20","09:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363900119260001",null,"L-2940076 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106936039","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-10-28","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01501455","Sample-Routine","Water","Groundwater","2015-05-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-314847083360301",null,"A-1410139 VOCs HAVE 2 DROPS HCL EACH VIAL",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-100758560","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-23","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01500565","Sample-Routine","Water","Groundwater","2015-05-21","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-425651070573701",null,"L-1470091 Samples were received chilled at the WHOI lab.","Bedrock","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-100718009","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01502117","Sample-Routine","Water","Groundwater","2015-04-30","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313613093510101",null,"L-1210145 GCVs btl condition changed to improper preservation, JNV  pH & alkalinity added, AM Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-100506503","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-09","improper preservationsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01501813","Sample-Routine","Water","Groundwater","2015-06-18","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-323318082202301",null,"L-1700047 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-101204708","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01501356","Sample-Routine","Water","Groundwater","2015-01-14","09:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-295358095374101",null,"L-0150042 Updated SID from 29538095374101 per Ging.  KB 4/2/15",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-100001589","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-01-23","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01502876","Sample-Routine","Water","Groundwater","2015-03-24","12:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-355000119230001",null,"L-0850129 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112110378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-01","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500782","Sample-Routine","Water","Groundwater","2015-08-05","10:00:00","CDT",{"$nulls":4},30.5,"feet",null,32.9,"feet",37.9,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-383214089571501",null,"A-2180043 Alternate contact - Kelly Warner (klwarner) 217-328-09727 5 drops HCL for VOC  (alternate contact-Kelly Warner, klwarner@usgs.gov, 217-328-9725). Acidified with HNO3. Acidified with HNO3. RADCHEM-acidified HNO3","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101495460","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-11","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500584","Sample-Routine","Water","Groundwater","2015-03-11","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-281050082111001",null,"L-0720006 Received March 12, 2015  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109638416","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-03-14","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01601256","Sample-Routine","Water","Groundwater","2015-12-08","13:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292331098294501",null,"L-3430019 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-103126279","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-11","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600292","Sample-Routine","Water","Groundwater","2015-11-03","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391400121200001",null,"L-3080126 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112113661","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-11-05","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01602052","Sample-Routine","Water","Groundwater","2016-02-10","17:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-290318098012101",null,"L-0430219 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103562889","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-19","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601450","Sample-Routine","Water","Groundwater","2016-08-09","11:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-460140118192801",null,"L-2230125 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-107475265","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-12",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601483","Sample-Routine","Water","Groundwater","2016-08-25","13:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-480638122125101",null,"L-2390142 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105626693","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-OR","USGS Oregon Water Science Center","nwisor.01.01700020","Sample-Routine","Water","Groundwater","2016-10-25","12:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-454827119173401",null,"L-3010032 X=improper sample container; LC1202 FU bottle has clear cap.  Samples were received chilled at the WHOI lab.  Changed proposal from CL16NAWOR to CL17NAWOR. 3/7/2017 MEC",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-106122625","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-10-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01700661","Quality Control Sample-Field Replicate","Water","Groundwater","2016-11-28","12:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-383450120334101",null,"L-3360041 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-112136676","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01601716","Sample-Routine","Water","Groundwater","2016-08-02","10:00:00","CDT",{"$nulls":4},22,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-450702093185101",null,"L-2160136 Please use more ice in cooler",null,"Not applicable","Not applicable",null,null,4080,"USGS parameter code 82398","Peristaltic pump",null,"Peristaltic pump","NWIS-105450867","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01700830","Sample-Routine","Water","Groundwater","2016-12-07","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371900118320001",null,"L-3440079 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-109453595","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601394","Sample-Routine","Water","Groundwater","2016-07-19","11:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-473827120044802",null,"L-2030303 Samples were received chilled at the WHOI lab. Added field pH per Huffman.  KB 8/4/16",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105285530","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01604344","Sample-Routine","Water","Groundwater","2016-07-13","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362021102045401",null,"L-1960214 One bottle for LC 1364 was empty upon receipt At ALS. Lid had broken  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105237336","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01601545","Sample-Routine","Water","Groundwater","2016-07-28","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Missouri Water Science Center","USGS-385222092544701",null,"L-2110157 Ok to analyze per wilson, KB 8/3/16 Samples were received unchilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105296395","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601409","Quality Control Sample-Field Replicate","Water","Groundwater","2016-07-13","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-461431119502001",null,"L-1960121 Samples were received chilled at the WHOI lab. Added fld alk per Huffman.  KB 8/15/16",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-107474649","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01605807","Sample-Routine","Water","Groundwater","2016-08-18","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373300122290001",null,"L-2320156 No tape on cap, cap loose - No leak or loss of sample Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108903749","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01601662","Sample-Routine","Water","Groundwater","2016-06-16","11:30:00","EDT",{"$nulls":6},"Below land-surface datum",163,"feet",244,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332146081582201",null,"L-1690025 VOC vials not numbered 1, 2 or 3. Changed Station Name from 30AA10 to 30AA09 per G. Gonthier. JCP 10/31/16  Changed Station Name from 30AA10 to 30AA09 per G. Gonthier. JCP 10/31/16",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-104843377","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01602335","Quality Control Sample-Field Replicate","Water","Groundwater","2016-03-14","14:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390400121070001",null,"L-0760037 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-112122712","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01602044","Sample-Routine","Water","Groundwater","2016-08-15","11:30:00","CDT",{"$nulls":4},9,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-450307093172301",{"$nulls":3},"Not applicable","Not applicable",null,null,4080,"USGS parameter code 82398","Peristaltic pump",null,"Peristaltic pump","NWIS-105734467","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01602043","Sample-Routine","Water","Groundwater","2016-08-15","14:00:00","CDT",{"$nulls":4},21.5,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-450557093201801",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible positive-pressure pump","NWIS-105734030","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01603731","Sample-Routine","Water","Groundwater","2016-06-14","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","TX001-354425101004405",null,"L-1670093 Changed Station ID to current per P. Ging. JPC 8/29/16  Loose cap on RA-224/RA-226 bottle. Approximately 60% lost. Changed Station ID to current per P. Ging. JPC 8/29/16  Samples were received chilled at the WHOI lab. Changed Station ID to current per P. Ging. JPC 8/29/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105055606","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01602054","Sample-Routine","Water","Groundwater","2016-03-08","16:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-291419098125101",null,"L-0700008 ID on bottle 291410988125101 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103563111","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01601034","Sample-Routine","Water","Groundwater","2016-09-07","14:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-424614083175300",null,"L-2520144 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4047,"USGS parameter code 82398","Submersible gear pump",null,"Submersible gear pump","NWIS-105794154","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01601655","Sample-Routine","Water","Groundwater","2016-06-14","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",161.42,"feet",222.42,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332216081583601",null,"L-1740132 X=GCV samples not labeled 1, 2, 3",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-104842536","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601671","Sample-Routine","Water","Groundwater","2016-02-09","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373905121011501",null,"L-0420034 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-106943313","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-19","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01602050","Sample-Routine","Water","Groundwater","2016-02-09","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-285317097421001",null,"L-0410076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103564701","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-19","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01601528","Sample-Routine","Water","Groundwater","2016-06-22","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-260725080162101",null,"L-1750343 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109255009","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601412","Quality Control Sample-Field Replicate","Water","Groundwater","2016-07-28","08:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-470727119113401",null,"L-2158712 Samples were received chilled at the WHOI lab.  Added user code WA and project chief RHUFFMAN. 8/4/2016 mec",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105337857","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601614","Sample-Routine","Water","Groundwater","2016-02-01","14:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390500121060001",null,"L-0340044 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112120303","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601385","Sample-Routine","Water","Groundwater","2016-01-28","13:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390100121070001",null,"L-0290034 X=one vial for LS4436 not received, one vial for LS4437 received empty  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112118266","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01601536","Sample-Routine","Water","Groundwater","2016-08-29","08:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-260056080125501",null,"L-2430080 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109259960","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01601982","Sample-Routine","Water","Groundwater","2016-08-24","09:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-414111084363200",null,"L-2380117 Place sample by sets in bag per ASR. Changed User Code from MI to OH per J. Giesen. JPC 9/1/16  Changed User Code from MI to OH per J. Giesen. JPC 9/1/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-105838043","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01800006","Sample-Routine","Water","Groundwater","2017-10-04","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363525109035201",null,"L-2780096 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108997934","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01706101","Sample-Routine","Water","Groundwater","2017-06-27","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-342100119180001",null,"L-1810226 Please do not put tape on GCC cap  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115684005","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01700452","Sample-Routine","Water","Groundwater","2017-07-12","09:30:00","MST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340718109181501",null,"L-1950270 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Submersible positive-pressure pump","NWIS-108200267","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01702967","Sample-Routine","Water","Groundwater","2017-07-10","11:20:00","MDT",{"$nulls":4},385,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Colorado Water Science Center","USEPA-371618107594201",null,"L-1920001 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108395461","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800025","Sample-Routine","Water","Groundwater","2017-10-10","06:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425944076385301",null,"L-2840042 Lab code 2689 changed to 2812 due to high solids",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108950229","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01700076","Sample-Routine","Water","Groundwater","2017-04-26","12:30:00","CDT",{"$nulls":4},23,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351217089560502",{"$nulls":3},"Not applicable","Not applicable",null,null,4047,"USGS parameter code 82398","Submersible gear pump",null,"Submersible gear pump","NWIS-107377344","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-04-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01701517","Sample-Routine","Water","Groundwater","2017-06-06","16:00:00","EDT",{"$nulls":6},"Below land-surface datum",163,"feet",244,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332146081582201",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-107786714","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700526","Sample-Routine","Water","Groundwater","2017-07-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392816075012101",null,"L-2349601 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108157406","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800067","Sample-Routine","Water","Groundwater","2017-10-16","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431635075310401",null,"L-2900040 Deleted Schedule 1307 per Murtagh. 11/3/2017 mec",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-109009119","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-19",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01700662","Sample-Routine","Water","Groundwater","2017-06-27","09:30:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-424748114443401",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-107973890","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01702928","Quality Control Sample-Field Replicate","Water","Groundwater","2017-02-21","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-334400116160001",null,"L-1388705 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-110780643","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-02-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707677","Sample-Routine","Water","Groundwater","2017-09-12","14:00:00","PDT",{"$nulls":4},160,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-384455121292101",null,"L-2560095 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110970496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700710","Sample-Routine","Water","Groundwater","2017-09-11","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393946074582901",null,"L-2550017 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-108691717","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703756","Sample-Routine","Water","Groundwater","2017-06-07","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302646099481501",null,"L-1590298 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108587112","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01702006","Sample-Routine","Water","Groundwater","2017-01-24","13:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340700117240001",null,"L-0270006 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109466780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-02-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01702623","Sample-Routine","Water","Groundwater","2017-08-30","09:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420224076041001",null,"L-2430074 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-108700316","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700660","Sample-Routine","Water","Groundwater","2017-08-23","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394342075040301",null,"L-2360181 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-108622135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01702580","Sample-Routine","Water","Groundwater","2017-07-31","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-421628076172801",null,"L-2140133 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-108697178","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01702717","Sample-Routine","Water","Groundwater","2017-06-28","11:00:00","MDT",{"$nulls":4},100,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Colorado Water Science Center","USEPA-380549107453301",null,"L-1840017 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108127064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703745","Sample-Routine","Water","Groundwater","2017-07-12","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311346100495601",null,"L-1940235 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108590328","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800646","Sample-Routine","Water","Groundwater","2017-12-04","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-353830120215001",null,"L-3410062 Added District Contact per S. Dugan. JPC 12/7/17  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115694641","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-12-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700461","Sample-Routine","Water","Groundwater","2017-06-19","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394255075030401",null,"L-2059601 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107897603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800079","Sample-Routine","Water","Groundwater","2017-10-24","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424619077122701",null,"L-2980007 GCV's btl conditoin changed to improper preservation, JNV  Lab code 2689 changed to 2812 due to high solids",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-109041832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01701513","Sample-Routine","Water","Groundwater","2017-06-06","09:00:00","EDT",{"$nulls":6},"Below land-surface datum",161.42,"feet",222.42,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332216081583601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107786216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01702421","Sample-Routine","Water","Groundwater","2017-06-26","12:00:00","MDT",{"$nulls":4},567,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Colorado Water Science Center","USGS-392554107195201",null,"L-1790003 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108012923","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800520","Sample-Routine","Water","Groundwater","2017-11-14","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382231120583401",null,"L-3200142 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110975906","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-11-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WY","USGS Wyoming Water Science Center","nwiswy.01.01700382","Sample-Routine","Water","Groundwater","2017-08-30","09:30:00","MDT",{"$nulls":4},221,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-414057108471501",null,"L-2430011 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-108647386","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800920","Sample-Routine","Water","Groundwater","2018-08-01","15:05:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-481205102514701",null,"L-2198718 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111575157","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01901135","Sample-Routine","Water","Groundwater","2018-12-18","09:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-400237122061101",null,"L-3530052 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-118294490","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-12-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01800927","Sample-Routine","Water","Groundwater","2018-09-17","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393035074533601",null,"L-2610069 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible centrifugal pump","NWIS-111828227","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01900001","Sample-Routine","Water","Groundwater","2018-10-03","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392045075021201",null,"L-2770114 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible centrifugal pump","NWIS-111973591","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-10-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01800774","Sample-Routine","Water","Groundwater","2018-08-07","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-395618074223501",null,"L-2200071 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not determined","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible centrifugal pump","NWIS-111518491","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01801656","Sample-Routine","Water","Groundwater","2018-03-13","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-293745098162001",null,"L-0730036 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110505318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01801536","Quality Control Sample-Field Replicate","Water","Groundwater","2018-01-30","13:50:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345255116361901",null,"L-0330022 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115936574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-02-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01804342","Sample-Routine","Water","Groundwater","2018-06-05","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365747120034901",null,"L-2568708 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-116034608","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802025","Sample-Routine","Water","Groundwater","2018-02-26","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345455117052601",null,"L-0600042 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116128032","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01801599","Sample-Routine","Water","Groundwater","2018-06-06","15:30:00","EDT",{"$nulls":6},"Below land-surface datum",163,"feet",244,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332146081582201",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-111064235","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01900338","Sample-Routine","Water","Groundwater","2018-10-23","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340742116053201",null,"L-2990163 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-118324607","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01801443","Sample-Routine","Water","Groundwater","2018-01-25","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363531121512601",null,"L-1648738 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115696187","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-02-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01803479","Sample-Routine","Water","Groundwater","2018-09-26","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-432652075121601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-111943822","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802942","Sample-Routine","Water","Groundwater","2018-04-05","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370145121560101",null,"L-1638708 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115702173","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":9},"The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-04-27","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01805429","Sample-Routine","Water","Groundwater","2018-08-14","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394800121350001",null,"L-2290048 Add District Contact, RHKENT to the ASR per R. Kent.  KMS, 8/22/18  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-118320912","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01801265","Quality Control Sample-Field Replicate","Water","Groundwater","2018-07-25","10:05:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-385536097071401",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-111385117","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-07-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802285","Sample-Routine","Water","Groundwater","2018-03-19","15:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345551116520801",null,"L-0820077 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-115700757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800933","Quality Control Sample-Field Replicate","Water","Groundwater","2018-08-07","16:25:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-455601101525101",null,"L-2220093 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-119325209","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800728","Sample-Routine","Water","Groundwater","2018-07-18","13:30:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-475952103590601",null,"L-2198703 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111319950","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-07-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01805431","Sample-Routine","Water","Groundwater","2018-08-13","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385300121150001",null,"L-2290050 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118320394","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-08-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01902228","Quality Control Sample-Field Replicate","Water","Groundwater","2019-07-30","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393455084180600",null,"L-2120132 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117421480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902235","Sample-Routine","Water","Groundwater","2019-06-27","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-415600071022501",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117242089","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-10",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01901970","Sample-Routine","Water","Groundwater","2019-07-23","16:00:00","EDT",{"$nulls":6},"Below land-surface datum",169.58,"feet",230.58,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332159081582501",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-117308180","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02000781","Sample-Routine","Water","Groundwater","2019-12-05","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381906122274901",null,"L-3400041 Remove GAMA from the program code per R Kent.  KMS, 12/9/19",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-119237535","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-12-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02000288","Sample-Routine","Water","Groundwater","2019-10-30","11:15:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-423156075232101",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-118065652","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000399","Sample-Routine","Water","Groundwater","2019-11-12","09:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-262000080110000",null,"L-3170037 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118429901","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906037","Sample-Routine","Water","Groundwater","2019-07-10","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380843121205201",null,"L-1970127 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118743846","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000351","Sample-Routine","Water","Groundwater","2019-10-31","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-264800081540001",null,"L-3050039 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118419830","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01902269","Sample-Routine","Water","Groundwater","2019-07-23","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USEPA-390502081475404",null,"L-2050176 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-117665226","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01903018","Quality Control Sample-Field Replicate","Water","Groundwater","2019-03-11","08:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-402018122255901",null,"L-0730001 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118301386","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-03-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000393","Sample-Routine","Water","Groundwater","2019-12-02","14:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-271300080180001",null,"L-3370083 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118428642","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-12-10",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000489","Sample-Routine","Water","Groundwater","2019-12-03","14:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-272104081023901",null,"L-3380007 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118454547","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-12-10",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902234","Sample-Routine","Water","Groundwater","2019-06-27","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-415541070443001",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117241882","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-10",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01902557","Sample-Routine","Water","Groundwater","2019-09-09","09:45:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-442045074064801",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117741599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01901486","Sample-Routine","Water","Groundwater","2019-06-05","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-423502071133001",null,"L-1578504 OK to login warm samples per J. Levitt. Chilled containers received warm at 11.8  Degrees C",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116840710","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-06-15","sample was warm when received",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-ME","USGS Maine Water Science Center","nwisma.01.01902830","Sample-Routine","Water","Groundwater","2019-09-10","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435010070142701",null,"L-2550071 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117738686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000378","Sample-Routine","Water","Groundwater","2019-10-29","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-262800081420001",null,"L-3030195 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible centrifugal pump","NWIS-118425500","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02000015","Sample-Routine","Water","Groundwater","2019-10-02","08:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-420123076221601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117873479","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02000279","Sample-Routine","Water","Groundwater","2019-10-21","11:15:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-422047075100201",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-118066611","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IN","USGS Indiana Water Science Center","nwisin.01.01901089","Sample-Routine","Water","Groundwater","2019-08-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","IN002-384400085240015",null,"MM-57850A",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Mulitple samplers used","NWIS-117754117","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01901972","Sample-Routine","Water","Groundwater","2019-07-24","10:30:00","EDT",{"$nulls":6},"Below land-surface datum",170,"feet",246,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332141081583601",null,"L-2060149 Updated SID Name from 30AA11 per G. Gonthier. JPC 10/11/19",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-117308427","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02001704","Sample-Routine","Water","Groundwater","2020-06-29","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",190,"feet",200,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332221081584601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-119296054","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001984","Sample-Routine","Water","Groundwater","2020-02-26","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-333537116135101",null,"L-0590108 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120714861","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-03-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001986","Sample-Routine","Water","Groundwater","2020-02-25","15:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-335650116383401",null,"L-0590110 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-120714567","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-03-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02004082","Quality Control Sample-Field Replicate","Water","Groundwater","2020-08-31","13:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340300117480001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-120699947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001988","Quality Control Sample-Field Replicate","Water","Groundwater","2020-02-25","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-333220115564401",null,"L-0590101 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120714269","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-03-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW02-VP-D001-052004-0","Sample","Air","Ambient Air","2004-05-20","15:40:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW02",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047849995.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-05-24",{"$nulls":3},5.6,"ppb",null,null,"STORET"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW04-VP-D004-052004-0","Sample","Air","Ambient Air","2004-05-23","10:54:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW04",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047851492.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-05-27",{"$nulls":3},6.8,"ppb",null,null,"STORET"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02001703","Sample-Routine","Water","Groundwater","2020-06-29","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",110,"feet",120,"feet",null,null,"USGS-National Water Quality Lab, Denver, CO","USGS-332221081584602",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-119296315","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120443R-gwdb","Sample-Other","Water","Groundwater","2013-08-01","15:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490947484",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",{"$f":"AP4704*1000","v":2},"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-04",{"$nulls":6},"2015-11-30T18:43:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120268R-gwdb","Sample-Other","Water","Groundwater","2013-08-01","12:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490859446",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",{"$f":"AP4729*1000","v":2},"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-04",{"$nulls":6},"2015-11-30T17:54:00","STORET"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100512","Sample-Routine","Water","Groundwater","2020-11-18","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-405200122150001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122573811","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-11-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120279.CHEM","Sample-Routine","Other",null,"2013-08-01","11:20:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-53578",64410,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725051519","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120279.CHEM/results/725051519/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2018-05-10T17:39:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120314.CHEM","Sample-Routine","Other",null,"2013-08-01","02:05:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-52553",62913,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.52445,-112.0817647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725053568","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120314.CHEM/results/725053568/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2018-05-10T17:39:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120442.CHEM","Sample-Routine","Other",null,"2013-08-01","02:35:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-58790",79323,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5244922,-112.0817217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725056945","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120442.CHEM/results/725056945/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2018-05-10T17:40:25","STORET"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003393","Sample-Routine","Water","Groundwater","2020-07-06","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380935121421601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-120693748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003097","Sample-Routine","Water","Groundwater","2020-06-23","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384224121261401",{"$nulls":3},"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-120691574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120478R-gwdb","Sample-Other","Water","Groundwater","2013-10-30","11:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769095",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",{"$f":"AP4856*1000","v":2},"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-11-03",{"$nulls":6},"2015-11-30T16:47:56","STORET"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001928","Sample-Routine","Water","Groundwater","2020-09-15","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-420927077471501",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119662911","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02002096","Sample-Routine","Water","Groundwater","2020-08-26","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-441703074294501",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119824988","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122139-gwdb","Sample-Routine","Water","Groundwater","2014-03-10","13:58:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64047","COP MW-48",{"$nulls":4},33.5008917,-112.1459333,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490875006",null,null,"1,3-Butadiene","Total",2,"ug/L",{"$f":"AP4920","v":2},"ug/l",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-14",{"$nulls":6},"2015-11-30T18:05:31","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122147-gwdb","Sample-Routine","Water","Groundwater","2014-03-11","10:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-59282","WCP-72M",{"$nulls":4},33.4994497,-112.1465058,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490871679",null,null,"1,3-Butadiene","Total",2,"ug/L",{"$f":"AP4945","v":2},"ug/l",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-14",{"$nulls":6},"2015-11-30T18:02:07","STORET"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100766","Sample-Routine","Water","Groundwater","2020-12-10","10:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390100121170001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122735817","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-12-12",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001780","Sample-Routine","Water","Groundwater","2020-08-18","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414504074355301",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119479031","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003815","Sample-Routine","Water","Groundwater","2020-08-20","09:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-353800120380001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-121370495","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001958","Sample-Routine","Water","Groundwater","2020-09-14","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425004077575501",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119716584","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-09-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122128-gwdb","Sample-Routine","Water","Groundwater","2014-03-06","09:40:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-59417","WCP-78",{"$nulls":4},33.5025417,-112.1515417,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491015285",null,null,"1,3-Butadiene","Total",2,"ug/L",{"$f":"AP5034","v":2},"ug/l",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-12",{"$nulls":6},"2015-11-30T19:16:20","STORET"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101589","Sample-Routine","Water","Groundwater","2021-01-26","10:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-372948120472801",null,"L-0290070 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-122462394","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02101722","Quality Control Sample-Field Replicate","Water","Groundwater","2021-06-29","14:00:00","EDT",{"$nulls":6},"Below land-surface datum",169.58,"feet",230.58,"feet",null,null,"U.S. Geological Survey-Water Resources Discipline","USGS-332159081582501",null,null,"Midville Aquifer System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121488119","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102890","Sample-Routine","Water","Groundwater","2021-04-12","13:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373828120444001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-123268668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-04-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101856","Sample-Routine","Water","Groundwater","2021-07-26","10:45:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-422833079095101",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"None","NWIS-121683973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02105572","Sample-Routine","Water","Groundwater","2021-08-31","08:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364800118110001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124414533","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-08","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02104679","Sample-Routine","Water","Groundwater","2021-07-14","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341400118130001",{"$nulls":3},"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-124426749","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02200441","Sample-Routine","Water","Groundwater","2021-11-16","10:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-383830120443801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124683023","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-11-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102571","Sample-Routine","Water","Groundwater","2021-03-30","15:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-351300119150001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-122875048","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-04-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102570","Sample-Routine","Water","Groundwater","2021-03-30","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-352600118560001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122874732","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-04-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02105359","Sample-Routine","Water","Groundwater","2021-08-25","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390339121214601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124419547","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-08","lab control sample (LCS) recovery outside of range or criteriasample was warm when received",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101900","Sample-Routine","Water","Groundwater","2021-07-26","07:15:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-420309078292001",null,"WQL-002142506",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-121773212","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101965","Sample-Routine","Water","Groundwater","2021-09-13","07:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431155077491401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-121900285","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02200193","Quality Control Sample-Field Replicate","Water","Groundwater","2021-11-01","15:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394144121274401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124416401","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-11-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02105363","Quality Control Sample-Field Replicate","Water","Groundwater","2021-08-17","13:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365600118140001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124418297","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-08-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02105199","Sample-Routine","Water","Groundwater","2021-08-12","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390018121264701",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124428614","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-08-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101966","Sample-Routine","Water","Groundwater","2021-09-13","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424235078323101",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-121900574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02101720","Sample-Routine","Water","Groundwater","2021-06-28","14:00:00","EDT",{"$nulls":4},65,"feet",null,110,"feet",120,"feet",null,null,"U.S. Geological Survey-Water Resources Discipline","USGS-332221081584602",null,null,"Dublin Aquifer System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121487851","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155338.CHEM","Sample-Routine","Other",null,"2016-08-09","08:25:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58754",79229,{"$nulls":4},32.2460544,-109.8368444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676181821","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-08-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155338.CHEM/results/676181821/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2017-11-03T10:08:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-150947.CHEM","Sample-Routine","Other",null,"2016-03-03","08:50:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59190",80594,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.492975,-113.1617631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707988435","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-03-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-150947.CHEM/results/707988435/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-03-13T10:39:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155331.CHEM","Sample-Routine","Other",null,"2016-09-14","10:48:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58747",79222,{"$nulls":4},32.2461081,-109.8364322,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676199676","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-09-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155331.CHEM/results/676199676/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2017-11-03T10:11:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155729.CHEM","Sample-Routine","Other",null,"2016-05-03","10:24:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59320",81183,{"$nulls":4},34.5619778,-112.4865694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676260446","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-05-09",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155729.CHEM/results/676260446/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2017-11-03T10:24:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156913.CHEM","Sample-Routine","Other",null,"2016-12-06","08:58:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59190",80594,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.492975,-113.1617631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993271","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156913.CHEM/results/707993271/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-03-13T10:41:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156922.CHEM","Sample-Routine","Other",null,"2016-12-05","01:43:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59189",80593,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4927864,-113.1616206,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993964","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156922.CHEM/results/707993964/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-03-13T10:41:18","STORET"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02300002","Sample-Routine","Water","Groundwater","2022-10-12","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-434729073582601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124560539","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-10-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156041.CHEM","Sample-Routine","Other",null,"2016-09-21","02:01:00","EST",{"$nulls":4},105,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","URS CONSULTANTS","AZDEQ_WPD-58793",79326,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.524588,-112.0825932,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725065646","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX","2016-09-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156041.CHEM/results/725065646/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-05-10T17:42:33","STORET"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02300018","Sample-Routine","Water","Groundwater","2022-10-05","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370520121340401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125800564","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-10-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155321.CHEM","Sample-Routine","Other",null,"2016-09-13","12:00:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58759",79234,{"$nulls":4},32.2459356,-109.8355467,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676198923","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-09-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155321.CHEM/results/676198923/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",null,"2017-11-03T10:11:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156252.CHEM","Sample-Routine","Other",null,"2016-10-21","12:20:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","URS CONSULTANTS","AZDEQ_WPD-56983",72800,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5244731,-112.0829683,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725065561","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX","2016-10-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156252.CHEM/results/725065561/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-05-10T17:42:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156916.CHEM","Sample-Routine","Other",null,"2016-12-06","11:46:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59187",80591,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4929192,-113.1616131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993502","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156916.CHEM/results/707993502/resdetectqntlmts","Laboratory Reporting Level",200,"ug/L",null,"2018-03-13T10:41:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-157559.CHEM","Sample-Routine","Other",null,"2017-02-20","03:12:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59320",81183,{"$nulls":4},34.5619778,-112.4865694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676159780","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2017-02-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-157559.CHEM/results/676159780/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2017-11-03T09:23:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18224.CHEM","Sample-Routine","Water",null,"2017-12-07","11:45:00","EST",{"$nulls":11},9725,"2017-WQARF SAMPLES","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-786710880","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18224.CHEM/results/786710880/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-05-01T10:07:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-157047.CHEM","Sample-Routine","Other",null,"2017-01-30","02:23:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59169",80492,{"$nulls":4},35.1904639,-109.4332189,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676161070","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2017-02-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-157047.CHEM/results/676161070/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2017-11-03T09:23:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18217.CHEM","Sample-Routine","Water",null,"2017-12-03","04:35:00","EST",{"$nulls":11},9725,"2017-WQARF SAMPLES","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-786710362","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18217.CHEM/results/786710362/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",null,"2019-05-01T10:07:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB11228.CHEM","Sample-Routine","Other",null,"2017-10-31","10:55:00","EST",{"$nulls":4},47,"ft",{"$nulls":5},9691,"VRP_0000","CH2M","AZDEQ_WPD-61636",81379,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.939721,-110.302651,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725240834","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"L | QA FLAGS: E8.",null,47,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"XENCO LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB11228.CHEM/results/725240834/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",null,"2018-05-15T09:02:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB05690.CHEM","Sample-Routine","Other",null,"2017-11-15","11:37:00","EST",{"$nulls":4},145,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725093105","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"G",null,145,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB05690.CHEM/results/725093105/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-05-11T10:34:12","STORET"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201685","Sample-Routine","Water","Groundwater","2022-08-11","08:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425457073521001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124824908","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-19","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203902","Sample-Routine","Water","Groundwater","2022-05-18","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-335224117332101",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-123652409","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-05-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02202672","Sample-Routine","Water","Groundwater","2022-03-16","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-351423119151201",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125813481","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-03-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.02200291","Quality Control Sample-Field Replicate","Water","Groundwater","2022-08-29","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361252077074501",null,"Data Quality Indicator (DQI) was changed Nov 2023 from \"U\" to \"S\" for parameter codes 52814, 52815, 52816, and 52817 per NWQL Tech Memo 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124274147","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14390.CHEM","Sample-Routine","Other",null,"2018-02-11","01:30:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61859",81549,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.2166806,-114.2024528,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734875908","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14390.CHEM/results/734875908/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2018-09-24T10:46:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14438.CHEM","Sample-Routine","Other",null,"2018-08-15","12:25:00","EST",{"$nulls":4},130,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734865744","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"G",null,130,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14438.CHEM/results/734865744/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2018-09-24T10:45:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14059.CHEM","Sample-Routine","Other",null,"2018-02-08","12:00:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61874",81564,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.6230583,-111.7158139,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734915947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14059.CHEM/results/734915947/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2018-09-24T10:51:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14057.CHEM","Sample-Routine","Other",null,"2018-05-24","10:45:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61925",81613,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},31.9654694,-110.2871444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734911912","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8,N1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14057.CHEM/results/734911912/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2018-09-24T10:51:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14072.CHEM","Sample-Routine","Other",null,"2018-02-02","03:30:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-52797",63335,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734875637","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: D2,E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14072.CHEM/results/734875637/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",null,"2018-09-24T10:46:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB17533.CHEM","Sample-Routine","Other",null,"2019-02-14","12:03:00","EST",{"$nulls":4},103.32,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-781050550","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"G",null,103.32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB17533.CHEM/results/781050550/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2019-03-28T10:25:27","STORET"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02201628","Sample-Routine","Water","Groundwater","2022-02-03","10:00:00","PST",{"$nulls":13},"USGS - California Water Science Center","USGS-351801118555801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125818681","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-02-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201692","Sample-Routine","Water","Groundwater","2022-09-28","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-440028073412701",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124823182","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.02200651","Sample-Routine","Water","Groundwater","2022-06-01","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-382439079344801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-123737390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.02200278","Sample-Routine","Water","Groundwater","2022-08-23","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342728077335701",null,"Data Quality Indicator (DQI) was changed Nov 2023 from \"U\" to \"S\" for parameter codes 52814, 52815, 52816, and 52817 per NWQL Tech Memo 2022.01",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-124209206","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.02300375","Sample-Routine","Water","Groundwater","2022-10-17","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-304819097361101",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124641599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-10-21","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203472","Sample-Routine","Water","Groundwater","2022-05-03","08:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340333117431001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-123532413","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-05-12",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.02200270","Sample-Routine","Water","Groundwater","2022-08-16","13:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351119076404801",null,"Data Quality Indicator (DQI) was changed Nov 2023 from \"U\" to \"S\" for parameter codes 52814, 52815, 52816, and 52817 per NWQL Tech Memo 2022.01",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-124163175","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.02200838","Sample-Routine","Water","Groundwater","2022-06-16","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380022079025601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124017236","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02202680","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-14","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341300119040001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-125238787","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-03-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.02300512","Sample-Routine","Water","Groundwater","2022-10-27","08:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-291828098485301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124691537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-11-07","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201696","Sample-Routine","Water","Groundwater","2022-08-30","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-430319073505701",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124824336","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02202784","Sample-Routine","Water","Groundwater","2022-03-28","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341400118590001",{"$nulls":3},"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-125235856","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-04-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201701","Sample-Routine","Water","Groundwater","2022-08-16","09:15:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-422744076164001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124821213","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-19","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02302043","Quality Control Sample-Field Replicate","Water","Groundwater","2023-08-16","11:00:00","EDT",{"$nulls":13},"U.S. Geological Survey","USGS-332146081590601",null,null,"Midville Aquifer System","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-126082231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.02301792","Sample-Routine","Water","Groundwater","2023-07-31","10:30:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-403413075064601",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-126005416","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-09","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.02301109","Sample-Routine","Water","Groundwater","2023-08-09","13:00:00","AST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-470850119323501",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-126378809","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["USGS-IN","USGS Indiana Water Science Center","nwisin.01.02300574","Quality Control Sample-Field Replicate","Water","Groundwater","2023-07-12","10:45:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-413312087223101",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-125884505","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-07-20","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",null,null,"NWIS"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132071-gwdb","Sample-Routine","Water","Groundwater","2012-12-27","11:12:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79224","ADEQ MW-104",{"$nulls":4},32.2460894,-109.8361219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491216465","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":9},"Qualifier:   MATRIX SPIKE:  MATRIX SPIKE RECOVERY WAS HIGH, THE METHOD CONTROL SAMPLE ASSOCIATED BLANK SPIKE RECOVERY WAS ACCEPTABLE",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2012-12-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132071-gwdb/results/491216465/resdetectqntlmts","Lower Reporting Limit",0.1,"mg/L",null,"2015-12-01T12:48:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47782.CHEM","Sample-Routine","Water","Groundwater","2021-10-20","09:17:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62530",81967,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5257528,-112.0818085,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-979418149","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47782.CHEM/results/979418149/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-06-26T10:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47811.CHEM","Sample-Routine","Water","Groundwater","2021-10-21","08:20:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63168",82487,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5275367,-112.0809018,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-979420295","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47811.CHEM/results/979420295/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-06-26T10:50:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47559.CHEM","Sample-Routine","Water","Groundwater","2022-04-29","08:50:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55524",68578,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5003333,-112.1428947,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992988156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47559.CHEM/results/992988156/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:46:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48412.CHEM","Sample-Routine","Water","Groundwater","2022-02-09","02:15:00","MST",{"$nulls":4},177,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62065",81675,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6930242,-114.6205641,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993007211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},177,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48412.CHEM/results/993007211/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48389.CHEM","Sample-Routine","Water","Groundwater","2022-02-09","10:45:00","MST",{"$nulls":4},175,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62266",81767,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6944968,-114.6203508,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993006562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},175,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48389.CHEM/results/993006562/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48457.CHEM","Quality Control Sample-Equipment Blank","Water","Groundwater","2022-02-22","09:15:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-53578",64410,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993003570","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48457.CHEM/results/993003570/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48452.CHEM","Sample-Routine","Water","Groundwater","2022-02-22","09:40:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-58793",79326,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.524588,-112.0825932,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993002829","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48452.CHEM/results/993002829/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48387.CHEM","Sample-Routine","Water","Groundwater","2022-02-09","01:50:00","MST",{"$nulls":4},181,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62067",81677,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6938676,-114.6203393,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993006486","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},181,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48387.CHEM/results/993006486/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:47:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47549.CHEM","Sample-Routine","Water","Groundwater","2022-04-29","10:08:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48633",58445,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5002411,-112.1458394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992987413","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47549.CHEM/results/992987413/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",null,"2023-11-09T09:45:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29755.CHEM","Sample-Routine","Water","Groundwater","2020-11-05","11:10:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52697",63127,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2015144,-110.9690139,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871461125","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29755.CHEM/results/871461125/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2020-12-28T09:35:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29930.CHEM","Sample-Routine","Water","Groundwater","2020-12-04","10:40:00","MST",{"$nulls":11},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62550",81985,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006402,-110.159209,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872129122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29930.CHEM/results/872129122/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2021-01-12T11:32:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36427.CHEM","Sample-Routine","Water","Groundwater","2021-12-16","09:50:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62947",82313,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834915,-110.7765133,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937421661","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36427.CHEM/results/937421661/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:36:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35009.CHEM","Sample-Routine","Water","Groundwater","2021-12-21","11:35:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52798",63336,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018136,-110.9687664,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994629166","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35009.CHEM/results/994629166/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:14:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40660.CHEM","Sample-Routine","Water","Groundwater","2021-12-20","12:03:00","MST",{"$nulls":4},39,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63527",82839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.915408,-110.1537148,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994667812","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},39,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40660.CHEM/results/994667812/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:18:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43695.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-14","12:00:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63287",82605,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.492633,-112.0111495,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992947444","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43695.CHEM/results/992947444/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43684.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","09:04:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992946630","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43684.CHEM/results/992946630/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35576.CHEM","Sample-Routine","Water","Groundwater","2021-09-21","08:50:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47010",56622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048881,-112.1491475,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933547117","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35576.CHEM/results/933547117/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-03-25T10:44:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34786.CHEM","Sample-Routine","Water","Groundwater","2021-11-19","03:35:00","MST",{"$nulls":11},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62551",81986,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9010599,-110.1597276,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992883603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34786.CHEM/results/992883603/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:35:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37344.CHEM","Sample-Routine","Water","Groundwater","2021-10-28","11:04:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943308120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37344.CHEM/results/943308120/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-07-05T13:15:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37318.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-29","03:23:00","MST",{"$nulls":4},49.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63126",82446,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7401428,-112.0096772,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943204118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},49.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37318.CHEM/results/943204118/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-06-29T01:16:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44907.CHEM","Sample-Routine","Water","Groundwater","2021-06-01","11:15:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58927",79646,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49344,-112.00216,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974186501","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44907.CHEM/results/974186501/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-05-05T10:06:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43709.CHEM","Sample-Routine","Water","Groundwater","2021-12-09","11:35:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992948480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43709.CHEM/results/992948480/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43728.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","12:54:00","MST",{"$nulls":4},83,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58933",79652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.495,-112.0034,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992949886","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},83,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43728.CHEM/results/992949886/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36490.CHEM","Sample-Routine","Water","Groundwater","2021-08-23","11:27:00","MST",{"$nulls":4},222,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62920",82290,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5401822,-112.1889801,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937425277","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: H1,R5,.",null,222,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36490.CHEM/results/937425277/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:37:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43683.CHEM","Sample-Routine","Water","Groundwater","2021-12-09","03:58:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58927",79646,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49344,-112.00216,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992946556","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43683.CHEM/results/992946556/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36435.CHEM","Sample-Routine","Water","Groundwater","2021-08-18","02:11:00","MST",{"$nulls":4},115.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62928",82297,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.1818502,-110.9567339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937422317","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36435.CHEM/results/937422317/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:36:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33320.CHEM","Sample-Routine","Water","Groundwater","2021-09-15","12:54:00","MST",{"$nulls":4},12,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62649",82056,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184502,-110.6848101,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916500822","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,12,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33320.CHEM/results/916500822/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2021-10-21T10:57:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43702.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","08:45:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62482",81929,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49491,-112.00217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992947962","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43702.CHEM/results/992947962/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44920.CHEM","Sample-Routine","Water","Groundwater","2021-05-26","07:46:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58931",79650,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4927,-112.00509,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974187509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44920.CHEM/results/974187509/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-05-05T10:08:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36454.CHEM","Sample-Routine","Water","Groundwater","2021-11-10","08:28:00","MST",{"$nulls":4},116,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62930",82299,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.1814244,-110.9569645,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937423723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},116,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36454.CHEM/results/937423723/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-03T12:37:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44929.CHEM","Sample-Routine","Water","Groundwater","2021-05-26","12:42:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974188205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44929.CHEM/results/974188205/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-05-05T10:09:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43720.CHEM","Sample-Routine","Water","Groundwater","2021-12-09","08:48:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62483",81930,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4953,-112.00041,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992949294","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43720.CHEM/results/992949294/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34181.CHEM","Sample-Routine","Water","Groundwater","2021-11-04","11:25:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62545",81980,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2121013,-112.7553064,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-925211110","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: R7.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34181.CHEM/results/925211110/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2021-12-28T10:27:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44879.CHEM","Sample-Routine","Water","Groundwater","2021-05-25","08:10:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974184332","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44879.CHEM/results/974184332/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-05-05T10:03:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43425.CHEM","Sample-Routine","Water","Groundwater","2021-11-18","11:30:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62812",82191,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5073158,-112.16763,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992938786","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43425.CHEM/results/992938786/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35197.CHEM","Sample-Routine","Water","Groundwater","2021-12-16","01:52:00","MST",{"$nulls":4},27,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49222",59152,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2213989,-114.5633969,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994629914","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,27,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35197.CHEM/results/994629914/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:14:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39211.CHEM","Sample-Routine","Water","Groundwater","2022-08-18","05:05:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-55722",69020,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7219444,-111.995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992910222","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39211.CHEM/results/992910222/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49220.CHEM","Sample-Routine","Water","Groundwater","2022-10-11","01:32:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-57301",74220,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5146417,-112.0740333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993022870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49220.CHEM/results/993022870/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:49:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35832.CHEM","Sample-Routine","Water","Groundwater","2022-03-10","10:25:00","MST",{"$nulls":4},6.1,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62854",82225,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2546474,-110.0311382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999646491","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},6.1,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35832.CHEM/results/999646491/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-18T09:29:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48943.CHEM","Sample-Routine","Water","Groundwater","2022-12-02","10:30:00","MST",{"$nulls":4},195,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63562",82869,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4991759,-112.1448776,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013462","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},195,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48943.CHEM/results/993013462/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39576.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","08:55:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63088",82414,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2859209,-110.1176133,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953666885","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39576.CHEM/results/953666885/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-10-12T10:05:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41613.CHEM","Sample-Routine","Water","Groundwater","2022-12-05","09:23:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62546",81981,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2122863,-112.7554876,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679080","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41613.CHEM/results/994679080/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:19:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40722.CHEM","Sample-Routine","Water","Groundwater","2022-03-31","01:00:00","MST",{"$nulls":4},400,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59144",80391,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4990642,-111.7194389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992919889","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},400,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40722.CHEM/results/992919889/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:38:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43657.CHEM","Sample-Routine","Water","Groundwater","2022-04-27","01:44:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63286",82604,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4925483,-112.0072941,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992944632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43657.CHEM/results/992944632/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41640.CHEM","Sample-Routine","Water","Groundwater","2022-11-29","02:06:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62951",82317,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833447,-110.7755438,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962655786","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41640.CHEM/results/962655786/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-01-06T10:31:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39203.CHEM","Sample-Routine","Water","Groundwater","2022-08-19","01:37:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62596",82030,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7236889,-111.9978667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992909630","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39203.CHEM/results/992909630/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41719.CHEM","Sample-Routine","Water","Groundwater","2022-03-23","07:53:00","MST",{"$nulls":4},240,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63496",82808,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4839139,-111.7258322,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992924824","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,240,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41719.CHEM/results/992924824/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45180.CHEM","Sample-Routine","Water","Groundwater","2022-10-17","12:34:00","MST",{"$nulls":4},170,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63288",82606,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4914866,-112.0080438,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992968998","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},170,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45180.CHEM/results/992968998/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:43:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38294.CHEM","Sample-Routine","Water","Groundwater","2022-03-02","04:48:00","MST",{"$nulls":4},216,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62914",82284,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5388505,-112.1868884,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943318567","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},216,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38294.CHEM/results/943318567/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-07-05T13:20:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42956.CHEM","Sample-Routine","Water","Groundwater","2022-09-08","11:45:00","MST",{"$nulls":4},61,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61604",81367,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5014952,-111.71389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992930857","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,61,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42956.CHEM/results/992930857/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38296.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-01","03:00:00","MST",{"$nulls":4},221,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62921",82291,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5402478,-112.1875664,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943318715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},221,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38296.CHEM/results/943318715/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-07-05T13:20:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36226.CHEM","Sample-Routine","Water","Groundwater","2022-03-15","03:09:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62373",81855,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2196725,-114.5646689,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994644570","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,15,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36226.CHEM/results/994644570/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43518.CHEM","Sample-Routine","Water","Groundwater","2022-08-09","03:38:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62689",82094,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4914188,-114.3478029,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992940414","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43518.CHEM/results/992940414/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39212.CHEM","Sample-Routine","Water","Groundwater","2022-08-18","06:35:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62565",81999,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.737457,-112.006639,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992910296","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39212.CHEM/results/992910296/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43341.CHEM","Sample-Routine","Water","Groundwater","2022-05-18","11:57:00","MST",{"$nulls":4},255,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63275",82593,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.499151,-112.1661915,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992937898","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},255,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43341.CHEM/results/992937898/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49205.CHEM","Sample-Routine","Water","Groundwater","2022-10-11","10:53:00","MST",{"$nulls":4},172,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62805",82184,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5147024,-112.074295,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993021760","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},172,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49205.CHEM/results/993021760/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:49:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40429.CHEM","Sample-Routine","Water","Groundwater","2022-04-20","11:55:00","MST",{"$nulls":4},14,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-62429",81905,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0683157,-112.1514167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999756930","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},14,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40429.CHEM/results/999756930/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-19T08:40:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43875.CHEM","Sample-Routine","Water","Groundwater","2022-11-17","10:21:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992952846","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43875.CHEM/results/992952846/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45257.CHEM","Sample-Routine","Water","Groundwater","2022-11-15","09:31:00","MST",{"$nulls":4},215,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63270",82588,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4975839,-112.1776579,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992973142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},215,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45257.CHEM/results/992973142/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:44:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43044.CHEM","Sample-Routine","Water","Groundwater","2022-11-05","02:06:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-55577",68658,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2290367,-110.9728622,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992933088","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43044.CHEM/results/992933088/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39219.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","01:45:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62567",82001,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7373778,-112.0074722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992910814","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39219.CHEM/results/992910814/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43871.CHEM","Sample-Routine","Water","Groundwater","2022-11-17","09:49:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992952550","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43871.CHEM/results/992952550/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39214.CHEM","Sample-Routine","Water","Groundwater","2022-08-19","09:59:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62679",82084,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7295278,-112.0061639,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992910444","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39214.CHEM/results/992910444/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38293.CHEM","Sample-Routine","Water","Groundwater","2022-03-02","02:24:00","MST",{"$nulls":4},216,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62916",82286,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5388076,-112.1871246,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943318493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},216,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38293.CHEM/results/943318493/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-07-05T13:20:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43681.CHEM","Sample-Routine","Water","Groundwater","2022-04-28","02:04:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63289",82607,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4899618,-112.008548,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992946408","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43681.CHEM/results/992946408/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:41:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39218.CHEM","Sample-Routine","Water","Groundwater","2022-08-18","01:05:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62579",82013,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7366333,-112.0075556,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992910740","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39218.CHEM/results/992910740/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41731.CHEM","Sample-Routine","Water","Groundwater","2022-03-24","12:57:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63223",82541,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4484,-111.732,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992925730","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41731.CHEM/results/992925730/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38512.CHEM","Sample-Routine","Water","Groundwater","2022-05-18","11:50:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49221",59151,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2194444,-114.5583333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994657274","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38512.CHEM/results/994657274/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:17:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36043.CHEM","Sample-Routine","Water","Groundwater","2022-03-03","02:25:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47014",56626,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048912,-112.1498029,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994643404","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36043.CHEM/results/994643404/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35830.CHEM","Sample-Routine","Water","Groundwater","2022-03-10","11:30:00","MST",{"$nulls":4},8.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62857",82228,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2552959,-110.0304703,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999646414","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},8.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35830.CHEM/results/999646414/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-18T09:29:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39188.CHEM","Sample-Routine","Water","Groundwater","2022-08-19","09:20:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62682",82087,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7311444,-112.0063889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39188.CHEM/results/992908520/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39207.CHEM","Sample-Routine","Water","Groundwater","2022-08-18","09:05:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-55703",68985,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7244444,-111.9983333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992909926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39207.CHEM/results/992909926/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41658.CHEM","Sample-Routine","Water","Groundwater","2022-11-23","12:25:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62687",82092,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7296278,-112.0082889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992921383","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41658.CHEM/results/992921383/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:38:51","STORET"]
["AZDEQ_GW","AZDEQ_GW","AZDEQ_GW-AB49488.CHEM","Sample-Routine","Water","Groundwater","2022-10-14","01:40:00","MST",{"$nulls":4},75,"ft",{"$nulls":5},9876,"2023_WQARF","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_GW-62506",81943,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4932191,-112.0156017,"Unknown","AZDEQ_GW","Unknown",null,"Miscellaneous (Other)","STORET-999445245","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_GW","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_GW/activities/AZDEQ_GW-AB49488.CHEM/results/999445245/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-16T10:09:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48822.CHEM","Sample-Routine","Water","Groundwater","2022-08-29","06:10:00","MST",{"$nulls":4},140,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62059",81669,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6941941,-114.6203401,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993010947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},140,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48822.CHEM/results/993010947/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49120.CHEM","Sample-Routine","Water","Groundwater","2022-09-20","05:53:00","MST",{"$nulls":4},140,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62776",82155,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.485781,-112.1016998,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993015544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},140,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49120.CHEM/results/993015544/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43514.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","10:15:00","MST",{"$nulls":4},120,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63290",82608,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4916875,-114.3496163,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992940118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},120,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43514.CHEM/results/992940118/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39183.CHEM","Sample-Routine","Water","Groundwater","2022-08-16","04:25:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-55717",69005,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7377778,-112.0077778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39183.CHEM/results/992908150/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38582.CHEM","Sample-Routine","Water","Groundwater","2022-06-07","02:48:00","MST",{"$nulls":4},10.9,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62855",82226,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2545888,-110.0306365,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994656309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},10.9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38582.CHEM/results/994656309/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:17:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36516.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-04-06","11:37:00","MST",{"$nulls":4},26,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63078",82406,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.5066308,-109.3643101,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937787599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},26,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36516.CHEM/results/937787599/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-05-05T10:33:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38966.CHEM","Sample-Routine","Water","Groundwater","2022-03-30","10:40:00","MST",{"$nulls":4},67,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62949",82315,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3831299,-110.7759143,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-950634152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},67,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38966.CHEM/results/950634152/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2022-08-30T11:00:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43331.CHEM","Sample-Routine","Water","Groundwater","2022-05-17","03:32:00","MST",{"$nulls":4},215,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63270",82588,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4975839,-112.1776579,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992937158","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},215,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43331.CHEM/results/992937158/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45179.CHEM","Sample-Routine","Water","Groundwater","2022-10-19","12:24:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992968924","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45179.CHEM/results/992968924/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:43:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47972.CHEM","Sample-Routine","Water","Groundwater","2022-10-03","12:35:00","MST",{"$nulls":4},162,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62517",81954,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5257535,-112.08189,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999652651","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},162,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47972.CHEM/results/999652651/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-18T09:30:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48820.CHEM","Sample-Routine","Water","Groundwater","2022-08-29","01:55:00","MST",{"$nulls":4},175,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62276",81777,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6930332,-114.6196025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999762231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},175,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48820.CHEM/results/999762231/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-19T08:41:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43647.CHEM","Sample-Routine","Water","Groundwater","2022-04-28","08:47:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63284",82602,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4929743,-112.0074929,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992943892","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43647.CHEM/results/992943892/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42922.CHEM","Sample-Routine","Water","Groundwater","2022-07-14","11:12:00","MST",{"$nulls":4},278,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-46019",51323,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4789453,-111.7301886,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992927760","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,278,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42922.CHEM/results/992927760/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37030.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-05-10","12:00:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47013",56625,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481143,-112.1492127,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994649345","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37030.CHEM/results/994649345/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:16:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48006.CHEM","Sample-Routine","Water","Groundwater","2022-10-04","01:05:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62161",81716,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5249138,-112.0816383,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999653927","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48006.CHEM/results/999653927/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-18T09:30:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35774.CHEM","Sample-Routine","Water","Groundwater","2022-02-15","10:53:00","MST",{"$nulls":4},27,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49222",59152,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2213989,-114.5633969,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994638800","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: R7.",null,27,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35774.CHEM/results/994638800/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:15:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39179.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","02:15:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62687",82092,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7296278,-112.0082889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992907854","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39179.CHEM/results/992907854/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:37:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37116.CHEM","Sample-Routine","Water","Groundwater","2022-05-20","11:18:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52801",63340,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016578,-110.9687681,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994653145","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37116.CHEM/results/994653145/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-12-04T10:17:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41724.CHEM","Sample-Routine","Water","Groundwater","2022-03-24","08:56:00","MST",{"$nulls":4},340,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63497",82809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4393639,-111.7067609,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992925202","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,340,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41724.CHEM/results/992925202/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47989.CHEM","Sample-Routine","Water","Groundwater","2022-10-04","12:40:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62162",81717,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5249151,-112.0816389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992992357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47989.CHEM/results/992992357/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:46:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43637.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-04-28","12:42:00","MST",{"$nulls":4},170,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63288",82606,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4914866,-112.0080438,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992943152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},170,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43637.CHEM/results/992943152/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:40:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43038.CHEM","Sample-Routine","Water","Groundwater","2022-11-05","12:48:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-55580",68661,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271119,-110.9671969,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992932644","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43038.CHEM/results/992932644/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:39:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48974.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-01-17","11:40:00","MST",{"$nulls":4},141,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62774",82153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4868778,-112.1006288,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993014508","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},141,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48974.CHEM/results/993014508/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49023.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","01:55:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62234",81738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4949968,-112.0012566,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993019984","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49023.CHEM/results/993019984/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:49:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48078.CHEM","Sample-Routine","Water","Groundwater","2023-01-25","03:15:00","MST",{"$nulls":4},153,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62557",81992,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6951457,-114.6203806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992995115","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},153,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48078.CHEM/results/992995115/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:46:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49000.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","02:15:00","MST",{"$nulls":4},105,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62234",81738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4949968,-112.0012566,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993018282","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},105,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49000.CHEM/results/993018282/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:48:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46327.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","10:20:00","MST",{"$nulls":4},164,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63622",82913,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49985,-112.146713,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992978963","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},164,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46327.CHEM/results/992978963/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:45:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45324.CHEM","Sample-Routine","Water","Groundwater","2023-03-30","02:56:00","MST",{"$nulls":4},55,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63125",82445,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7398811,-112.0098944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974803569","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},55,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45324.CHEM/results/974803569/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-05-23T13:51:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49041.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","02:30:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62234",81738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4949968,-112.0012566,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993021316","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49041.CHEM/results/993021316/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:49:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46324.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","11:10:00","MST",{"$nulls":4},268,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-49413",59282,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4994497,-112.1465058,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992978741","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},268,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46324.CHEM/results/992978741/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:45:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48563.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","10:40:00","MST",{"$nulls":4},181,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55494",68499,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945844,-114.6232625,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999760933","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,181,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48563.CHEM/results/999760933/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2024-01-19T08:41:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46342.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-04-26","10:05:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62953",82319,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833686,-110.7763725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983661884","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46342.CHEM/results/983661884/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-07-26T11:00:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48555.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","08:55:00","MST",{"$nulls":4},95,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55379",68280,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6933111,-114.6211361,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993000150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},95,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48555.CHEM/results/993000150/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:47:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48571.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","01:45:00","MST",{"$nulls":4},159,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-15970",24732,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6941992,-114.6281436,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993001343","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,159,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48571.CHEM/results/993001343/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",null,"2023-11-09T09:47:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29973.CHEM","Sample-Routine","Water","Groundwater","2019-01-30","11:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62353",81849,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7359623,-112.0089103,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872412442","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29973.CHEM/results/872412442/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2021-01-19T10:33:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26153.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","03:11:00","MST",{"$nulls":4},210,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62400",81882,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4270989,-112.0871484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832561871","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},210,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26153.CHEM/results/832561871/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-07T11:05:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB24946.CHEM","Sample-Routine","Water","Groundwater","2019-09-18","01:53:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-51313",61442,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4276056,-112.088,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-824334440","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB24946.CHEM/results/824334440/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-02-25T09:36:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26147.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","10:19:00","MST",{"$nulls":4},146,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-58425",78221,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4330189,-112.0983989,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832560765","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},146,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26147.CHEM/results/832560765/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-07T11:05:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26352.CHEM","Sample-Routine","Water","Groundwater","2020-03-11","12:10:00","MST",{"$nulls":4},215,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62401",81883,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4289567,-112.0911729,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839248111","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},215,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26352.CHEM/results/839248111/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-22T09:30:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26371.CHEM","Sample-Routine","Water","Groundwater","2020-03-11","11:30:00","MST",{"$nulls":4},185,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62401",81883,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4289567,-112.0911729,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839248190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},185,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26371.CHEM/results/839248190/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-22T09:30:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26354.CHEM","Sample-Routine","Water","Groundwater","2020-03-11","11:45:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62401",81883,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4289567,-112.0911729,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839248664","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26354.CHEM/results/839248664/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",null,"2020-04-22T09:30:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48317.CHEM","Sample-Routine","Water","Groundwater","2021-11-17","09:30:00","MST",{"$nulls":4},65,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63191",82510,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7237579,-112.00439,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993004700","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},65,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48317.CHEM/results/993004700/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2023-11-09T09:47:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49846.CHEM","Sample-Routine","Water","Groundwater","2022-02-18","10:45:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62524",81961,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.525762,-112.081192,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993027081","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49846.CHEM/results/993027081/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2023-11-09T09:49:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49844.CHEM","Sample-Routine","Water","Groundwater","2022-02-17","01:00:00","MST",{"$nulls":4},228,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63147",82466,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5192175,-112.0814893,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999764295","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,228,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49844.CHEM/results/999764295/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",null,"2024-01-19T08:41:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35584.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","08:13:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63058",82392,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482178,-112.1488252,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933547717","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35584.CHEM/results/933547717/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",null,"2022-03-25T10:44:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48830.CHEM","Sample-Routine","Water","Groundwater","2022-08-30","04:50:00","MST",{"$nulls":4},148,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61904",81592,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6940346,-114.6214261,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993011475","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},148,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48830.CHEM/results/993011475/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",null,"2023-11-09T09:48:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47548.CHEM","Sample-Routine","Water","Groundwater","2022-04-29","07:15:00","MST",{"$nulls":4},154,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59248",81049,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4990011,-112.1439503,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992987339","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},154,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47548.CHEM/results/992987339/resdetectqntlmts","Laboratory Reporting Level",1.49000000953674,"ug/L",null,"2023-11-09T09:45:55","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150782-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","14:50:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79954","THOMPSON SMP-1",{"$nulls":4},34.9024408,-110.1635669,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552063372","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150782-gwdb/results/552063372/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",null,"2016-05-12T02:27:45","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146165-gwdb","Sample-Routine","Water","Groundwater","2015-03-12","12:05:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-58228","IRA-10-230",{"$nulls":4},32.2807097,-110.9995278,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552027559","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-18",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146165-gwdb/results/552027559/resdetectqntlmts","Method Detection Level",2,"ug/L",null,"2016-05-12T02:07:13","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150572-gwdb","Sample-Routine","Water","Groundwater","2015-12-03","10:27:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80597","MW-6A",{"$nulls":4},33.4928372,-113.1617644,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552116258","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-11",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150572-gwdb/results/552116258/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",null,"2016-05-12T02:51:21","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146166-gwdb","Sample-Routine","Water","Groundwater","2015-03-12","13:53:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-58234","IRA-5",{"$nulls":4},32.2810203,-111.0101806,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552100954","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-18",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146166-gwdb/results/552100954/resdetectqntlmts","Method Detection Level",2,"ug/L",null,"2016-05-12T02:44:03","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150955-gwdb","Sample-Routine","Water","Groundwater","2016-03-03","12:10:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80595","MW-4",{"$nulls":4},33.4930494,-113.16208,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552047643","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150955-gwdb/results/552047643/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",null,"2016-05-12T02:21:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29740.CHEM","Sample-Routine","Water","Groundwater","2019-12-13","09:45:00","MST",{"$nulls":4},330,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62097",81696,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2270973,-110.8359018,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871403139","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,330,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29740.CHEM/results/871403139/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2020-12-24T10:58:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB22361.CHEM","Sample-Routine","Water","Groundwater","2019-08-09","09:00:00","EST",{"$nulls":4},333,"ft",{"$nulls":5},9749,"2018-WQARF Samples","AMEC EARTH AND ENVIRONMENTAL","AZDEQ_WPD-62133",81708,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2271694,-110.8374424,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-797209543","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,333,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB22361.CHEM/results/797209543/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2019-08-30T13:02:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18569.CHEM","Sample-Routine","Water","Groundwater","2019-05-01","12:15:00","EST",{"$nulls":4},316,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50534",60649,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2331389,-110.84327,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-788807477","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,316,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18569.CHEM/results/788807477/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2019-06-07T09:23:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29750.CHEM","Sample-Routine","Water","Groundwater","2019-12-13","08:55:00","MST",{"$nulls":4},320,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62133",81708,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271694,-110.8374424,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871403839","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,320,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29750.CHEM/results/871403839/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2020-12-24T10:58:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30405.CHEM","Sample-Routine","Water","Groundwater","2019-11-18","08:53:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","ARIZONA DEPT OF ENVIRONMENTAL QUALITY","AZDEQ_WPD-55006",67110,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3105556,-111.0305556,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-875256041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30405.CHEM/results/875256041/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2021-02-08T10:56:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28829.CHEM","Sample-Routine","Water","Groundwater","2020-08-06","06:35:00","MST",{"$nulls":4},14,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-57686",75280,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2564885,-114.1467892,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-855758198","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,14,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28829.CHEM/results/855758198/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2020-09-08T11:01:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28201.CHEM","Sample-Routine","Water","Groundwater","2020-06-02","01:12:00","MST",{"$nulls":4},18.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62451",81923,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2561252,-114.1466311,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849902581","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,18.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28201.CHEM/results/849902581/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2020-06-25T09:43:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26758.CHEM","Sample-Routine","Water","Groundwater","2020-04-07","09:10:00","MST",{"$nulls":4},181,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-59280",81234,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3689967,-111.8173992,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-844184173","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,181,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26758.CHEM/results/844184173/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2020-04-27T15:05:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35355.CHEM","Sample-Routine","Water","Groundwater","2021-12-22","01:30:00","MST",{"$nulls":4},101,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63015",82379,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8792315,-111.7358321,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994635424","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,101,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35355.CHEM/results/994635424/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2023-12-04T10:15:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44712.CHEM","Sample-Routine","Water","Groundwater","2023-02-14","11:00:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","ARIZONA DEPT OF ENVIRONMENTAL QUALITY","AZDEQ_WPD-62964",82330,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6990297,-114.6711554,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999759512","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44712.CHEM/results/999759512/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",null,"2024-01-19T08:41:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38278.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","11:02:00","MST",{"$nulls":4},34.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63104",82430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2858486,-110.1177657,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943318419","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},34.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38278.CHEM/results/943318419/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2022-07-05T13:20:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40265.CHEM","Sample-Routine","Water","Groundwater","2022-09-22","09:23:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62777",82156,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2127512,-112.7555304,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956947825","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40265.CHEM/results/956947825/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2022-10-28T11:00:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48176.CHEM","Sample-Routine","Water","Groundwater","2023-01-31","07:43:00","MST",{"$nulls":4},165,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61907",81595,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6943898,-114.6224328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999654458","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},165,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48176.CHEM/results/999654458/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",null,"2024-01-18T09:31:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48146.CHEM","Sample-Routine","Water","Groundwater","2022-05-11","11:40:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63198",82517,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7362643,-112.0104013,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999657596","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48146.CHEM/results/999657596/resdetectqntlmts","Laboratory Reporting Level",2.99000000953674,"ug/L",null,"2024-01-18T09:31:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25019.CHEM","Sample-Routine","Water","Groundwater","2019-11-22","11:28:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52797",63335,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-827751038","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25019.CHEM/results/827751038/resdetectqntlmts","Laboratory Reporting Level",3.3,"ug/L",null,"2020-03-13T11:23:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32888.CHEM","Sample-Routine","Water","Groundwater","2020-10-15","08:55:00","MST",{"$nulls":4},140,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-55116",67518,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3588022,-111.8017806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905983440","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,140,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32888.CHEM/results/905983440/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-08-03T09:45:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32881.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","09:26:00","MST",{"$nulls":4},330,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62097",81696,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2270973,-110.8359018,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905982929","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,330,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32881.CHEM/results/905982929/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-08-03T09:45:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29342.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","09:56:00","MST",{"$nulls":4},260,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62246",81749,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4795365,-112.0150513,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860619677","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,260,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29342.CHEM/results/860619677/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32872.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","10:13:00","MST",{"$nulls":4},370,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62096",81695,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2266833,-110.8375773,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905982272","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,370,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32872.CHEM/results/905982272/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-08-03T09:45:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29304.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","02:36:00","MST",{"$nulls":4},210,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62243",81746,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4873517,-112.0020122,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616497","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,210,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29304.CHEM/results/860616497/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29279.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","08:20:00","MST",{"$nulls":4},84.7,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56542",71385,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900806,-111.9946153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860614201","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,84.7,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29279.CHEM/results/860614201/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29711.CHEM","Sample-Routine","Water","Groundwater","2020-09-23","08:01:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-40430",46748,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4945336,-111.9822153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871302523","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29711.CHEM/results/871302523/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-12-22T12:17:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29279.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","08:20:00","MST",{"$nulls":4},84.7,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56542",71385,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900806,-111.9946153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860614202","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: H1.",null,84.7,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29279.CHEM/results/860614202/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2020-11-02T09:31:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32859.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","10:18:00","MST",{"$nulls":4},130,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50238",60341,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3780697,-111.8245025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905981688","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,130,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32859.CHEM/results/905981688/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-08-03T09:45:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33227.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","01:58:00","MST",{"$nulls":4},245,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62251",81754,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4716569,-112.0263153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916457921","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,245,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33227.CHEM/results/916457921/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:12:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33352.CHEM","Sample-Routine","Water","Groundwater","2021-09-01","07:11:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62876",82247,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560154,-114.1467932,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916470229","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5,V1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33352.CHEM/results/916470229/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:15:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33244.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","08:03:00","MST",{"$nulls":4},160,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916459475","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,160,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33244.CHEM/results/916459475/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:12:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34152.CHEM","Sample-Routine","Water","Groundwater","2021-11-29","02:22:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62894",82265,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2553765,-114.1463451,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994133126","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34152.CHEM/results/994133126/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-29T09:06:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33249.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","10:02:00","MST",{"$nulls":4},132,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62479",81926,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.48411,-112.00501,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916459845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,V1,L5.",null,132,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33249.CHEM/results/916459845/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:12:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33246.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","12:00:00","MST",{"$nulls":4},255,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62050",81661,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4765057,-112.0172709,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916459623","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,255,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33246.CHEM/results/916459623/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:12:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33065.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","08:01:00","MST",{"$nulls":4},48,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58419",78144,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4950028,-111.9802,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916455554","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,48,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33065.CHEM/results/916455554/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32915.CHEM","Sample-Routine","Water","Groundwater","2021-07-20","08:05:00","MST",{"$nulls":4},333,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-906967011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,N1.",null,333,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32915.CHEM/results/906967011/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-08-09T21:59:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33059.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","11:25:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58920",79629,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4924967,-111.9895194,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916455036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,45,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33059.CHEM/results/916455036/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:11:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33359.CHEM","Sample-Routine","Water","Groundwater","2021-08-31","12:44:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-57684",75260,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2561079,-114.146582,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916470873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5,V1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33359.CHEM/results/916470873/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2021-10-19T11:15:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37515.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","11:18:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50523",60638,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2325675,-110.862555,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902807","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,H1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37515.CHEM/results/992902807/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:37:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39496.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","03:05:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62247",81750,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4750136,-112.0119411,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992914465","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39496.CHEM/results/992914465/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:38:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43087.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","11:59:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62133",81708,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271694,-110.8374424,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992934049","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43087.CHEM/results/992934049/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:39:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39518.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","12:25:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992916093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39518.CHEM/results/992916093/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:38:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39487.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","09:40:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50243",60346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3780192,-111.8242253,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992911849","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39487.CHEM/results/992911849/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:37:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35497.CHEM","Sample-Routine","Water","Groundwater","2022-03-01","10:28:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62543",81978,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934,-111.9863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992884707","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: P,  | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35497.CHEM/results/992884707/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:35:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43090.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","07:40:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62132",81707,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272038,-110.8374429,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992934271","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43090.CHEM/results/992934271/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:39:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43112.CHEM","Sample-Routine","Water","Groundwater","2022-09-15","08:20:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","WSP USA ENVIRONMENT & INFRASTRUCTURE INC","AZDEQ_WPD-56712",72041,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3582617,-111.8110453,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992935899","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43112.CHEM/results/992935899/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:40:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35501.CHEM","Sample-Routine","Water","Groundwater","2022-03-01","10:39:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62544",81979,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934,-111.9863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992885008","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35501.CHEM/results/992885008/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:35:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38743.CHEM","Sample-Routine","Water","Groundwater","2022-07-20","11:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-47634",57289,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271944,-110.8376042,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992906225","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38743.CHEM/results/992906225/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",null,"2023-11-09T09:37:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147242-gwdb","Sample-Other","Water","Groundwater","2015-05-14","06:43:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-47724","MICROCHIP TECH MW-11",{"$nulls":4},33.4155147,-111.9696558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552127084","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":9},"Qualifier:   GENERAL:  SEE CASE NARRATIVE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Xenco Laboratories","2015-05-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147242-gwdb/results/552127084/resdetectqntlmts","Lower Reporting Limit",5,"ug/L",null,"2016-05-12T02:54:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34986.CHEM","Sample-Routine","Water","Groundwater","2021-12-03","12:39:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62654",82061,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0183911,-110.6841183,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994508244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34986.CHEM/results/994508244/resdetectqntlmts","Laboratory Reporting Level",5.98,"ug/L",null,"2023-12-02T11:38:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47987.CHEM","Sample-Routine","Water","Groundwater","2022-10-04","07:35:00","MST",{"$nulls":4},228,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63147",82466,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5192175,-112.0814893,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999653177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},228,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47987.CHEM/results/999653177/resdetectqntlmts","Laboratory Reporting Level",5.98,"ug/L",null,"2024-01-18T09:30:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39584.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","10:10:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63092",82418,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2861373,-110.1179947,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667477","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39584.CHEM/results/953667477/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",null,"2022-10-12T10:05:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37045.CHEM","Sample-Routine","Water","Groundwater","2022-05-12","03:25:00","MST",{"$nulls":4},19,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63065",82399,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481968,-112.1490371,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650481","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,19,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37045.CHEM/results/994650481/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",null,"2023-12-04T10:16:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34160.CHEM","Sample-Routine","Water","Groundwater","2021-11-30","10:40:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62876",82247,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560154,-114.1467932,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994246934","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8,D1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34160.CHEM/results/994246934/resdetectqntlmts","Laboratory Reporting Level",8,"ug/L",null,"2023-11-30T10:13:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34052.CHEM","Sample-Routine","Water","Groundwater","2021-11-09","08:51:00","MST",{"$nulls":4},216.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62822",82200,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7655507,-112.4536215,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-921314367","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,216.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34052.CHEM/results/921314367/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2021-12-06T09:10:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34772.CHEM","Sample-Routine","Water","Groundwater","2021-12-09","08:53:00","MST",{"$nulls":4},33.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62860",82231,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.255927,-110.0234277,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626375","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: Q7,T4.",null,33.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34772.CHEM/results/994626375/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:14:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34774.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","02:51:00","MST",{"$nulls":4},26.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62859",82230,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2558122,-110.0239078,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626505","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,26.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34774.CHEM/results/994626505/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:14:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41482.CHEM","Sample-Routine","Water","Groundwater","2022-12-05","11:06:00","MST",{"$nulls":4},207.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62824",82202,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7648219,-112.4536413,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994675649","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,207.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41482.CHEM/results/994675649/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:19:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39476.CHEM","Sample-Routine","Water","Groundwater","2022-09-06","04:38:00","MST",{"$nulls":4},36.8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62868",82239,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2528438,-110.0338152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663221","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,36.8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39476.CHEM/results/994663221/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:18:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43184.CHEM","Sample-Routine","Water","Groundwater","2022-11-10","09:13:00","MST",{"$nulls":4},24,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63058",82392,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482178,-112.1488252,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994683062","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,24,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43184.CHEM/results/994683062/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:19:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43198.CHEM","Sample-Routine","Water","Groundwater","2022-12-15","12:45:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63023",82387,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.879323,-111.7356152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994684324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43198.CHEM/results/994684324/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:19:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38263.CHEM","Sample-Routine","Water","Groundwater","2022-05-26","10:19:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63017",82381,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8793896,-111.735863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994654260","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38263.CHEM/results/994654260/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:17:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43788.CHEM","Sample-Routine","Water","Groundwater","2022-12-07","02:22:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62978",82344,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358918,-110.9416598,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994685299","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43788.CHEM/results/994685299/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:20:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41569.CHEM","Sample-Routine","Water","Groundwater","2022-12-08","10:06:00","MST",{"$nulls":4},13.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62857",82228,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2552959,-110.0304703,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994677703","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,13.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41569.CHEM/results/994677703/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:19:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43076.CHEM","Sample-Routine","Water","Groundwater","2022-12-28","09:30:00","MST",{"$nulls":4},8.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62866",82237,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530049,-110.0337858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994681622","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,Q7.",null,8.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43076.CHEM/results/994681622/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:19:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38479.CHEM","Sample-Routine","Water","Groundwater","2022-06-20","10:58:00","MST",{"$nulls":4},217,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62822",82200,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7655507,-112.4536215,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994655571","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,217,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38479.CHEM/results/994655571/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:17:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38474.CHEM","Sample-Routine","Water","Groundwater","2022-06-20","10:32:00","MST",{"$nulls":4},177.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62825",82203,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7648134,-112.4536487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994655252","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,177.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38474.CHEM/results/994655252/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:17:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41170.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-09-09","03:08:00","MST",{"$nulls":4},14,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63069",82403,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483984,-112.149587,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994670161","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,14,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41170.CHEM/results/994670161/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:18:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35257.CHEM","Sample-Routine","Water","Groundwater","2022-02-08","10:21:00","MST",{"$nulls":4},205.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62824",82202,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7648219,-112.4536413,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994632349","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,205.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35257.CHEM/results/994632349/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:14:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43786.CHEM","Sample-Routine","Water","Groundwater","2022-12-09","08:32:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62982",82348,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356701,-110.9417204,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994685147","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43786.CHEM/results/994685147/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:19:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46206.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-01-26","09:03:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47013",56625,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481143,-112.1492127,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994696497","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46206.CHEM/results/994696497/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:20:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45510.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","10:18:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62991",82357,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358759,-110.9421197,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994695903","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,36,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45510.CHEM/results/994695903/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:20:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49079.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","08:14:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63014",82378,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.879284,-111.7359009,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49079.CHEM/results/994704329/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49405.CHEM","Sample-Routine","Water","Groundwater","2023-06-14","05:07:00","MST",{"$nulls":4},12,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62866",82237,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530049,-110.0337858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983676142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,12,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49405.CHEM/results/983676142/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-07-26T11:01:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49081.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","09:25:00","MST",{"$nulls":4},102,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63016",82380,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8793638,-111.7360725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704477","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,102,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49081.CHEM/results/994704477/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",null,"2023-12-04T10:21:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35305.CHEM","Sample-Routine","Water","Groundwater","2021-09-28","11:13:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62989",82355,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359302,-110.9417269,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-932819491","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35305.CHEM/results/932819491/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",null,"2022-03-18T10:55:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35329.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-07","12:00:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62993",82359,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357048,-110.9417694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994634273","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35329.CHEM/results/994634273/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",null,"2023-12-04T10:15:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28827.CHEM","Sample-Routine","Water","Groundwater","2020-08-06","04:01:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62446",81918,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2559398,-114.1465297,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-855758050","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,D1.",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28827.CHEM/results/855758050/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2020-09-08T11:01:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28825.CHEM","Sample-Routine","Water","Groundwater","2020-08-06","05:30:00","MST",{"$nulls":4},18.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62451",81923,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2561252,-114.1466311,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-855757902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,D1.",null,18.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28825.CHEM/results/855757902/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2020-09-08T11:01:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34767.CHEM","Sample-Routine","Water","Groundwater","2021-12-06","04:05:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62865",82236,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530049,-110.0337858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D1,Q3,T4.",null,40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34767.CHEM/results/994626767/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:14:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33228.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","08:16:00","MST",{"$nulls":4},260,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916458064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: P,  | QA FLAGS: E8,D1,V1,L5.",null,260,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33228.CHEM/results/916458064/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2021-10-19T11:12:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34770.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","04:41:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62858",82229,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560194,-110.0236635,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626245","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,Q7,T4.",null,32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34770.CHEM/results/994626245/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:14:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33254.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","08:14:00","MST",{"$nulls":4},240,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916460215","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,D1,V1,L5.",null,240,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33254.CHEM/results/916460215/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2021-10-19T11:12:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43794.CHEM","Sample-Routine","Water","Groundwater","2022-12-09","09:47:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994685750","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43794.CHEM/results/994685750/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:20:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41563.CHEM","Sample-Routine","Water","Groundwater","2022-12-08","12:01:00","MST",{"$nulls":4},8.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62853",82224,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2541309,-110.0308096,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994677326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D1,T4.",null,8.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41563.CHEM/results/994677326/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:19:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38476.CHEM","Sample-Routine","Water","Groundwater","2022-06-20","11:57:00","MST",{"$nulls":4},159.6,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62817",82195,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651699,-112.4536728,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994655380","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,159.6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38476.CHEM/results/994655380/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:17:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41121.CHEM","Sample-Routine","Water","Groundwater","2022-11-08","09:47:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62858",82229,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560194,-110.0236635,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994669272","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41121.CHEM/results/994669272/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:18:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41180.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","02:12:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63070",82404,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0478107,-112.1488738,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994670909","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1.",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41180.CHEM/results/994670909/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:18:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44710.CHEM","Sample-Routine","Water","Groundwater","2023-02-14","12:00:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","ARIZONA DEPT OF ENVIRONMENTAL QUALITY","AZDEQ_WPD-62957",82323,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6991842,-114.6709662,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999759370","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44710.CHEM/results/999759370/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2024-01-19T08:41:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45493.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","02:21:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994694627","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1,.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45493.CHEM/results/994694627/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:20:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45165.CHEM","Sample-Routine","Water","Groundwater","2023-03-24","08:46:00","MST",{"$nulls":4},38,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62872",82243,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529809,-110.0338286,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974992472","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,38,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45165.CHEM/results/974992472/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-05-25T10:52:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44711.CHEM","Sample-Routine","Water","Groundwater","2023-02-14","10:18:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","ARIZONA DEPT OF ENVIRONMENTAL QUALITY","AZDEQ_WPD-62957",82323,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6991842,-114.6709662,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999759441","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44711.CHEM/results/999759441/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2024-01-19T08:41:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45505.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","03:24:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62989",82355,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359302,-110.9417269,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994695531","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1,.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45505.CHEM/results/994695531/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",null,"2023-12-04T10:20:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48426.CHEM","Sample-Routine","Water","Groundwater","2022-02-09","11:30:00","MST",{"$nulls":4},142,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55380",68281,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6932833,-114.6211361,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993007712","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},142,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48426.CHEM/results/993007712/resdetectqntlmts","Laboratory Reporting Level",29.8999996185303,"ug/L",null,"2023-11-09T09:48:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37313.CHEM","Sample-Routine","Water","Groundwater","2021-12-27","05:25:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63123",82443,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7400311,-112.0094914,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943203674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},45,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37313.CHEM/results/943203674/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-06-29T01:16:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35445.CHEM","Sample-Routine","Water","Groundwater","2021-09-28","01:35:00","MST",{"$nulls":4},19,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63063",82397,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0480503,-112.1488712,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933542595","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},19,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35445.CHEM/results/933542595/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-03-25T10:44:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33328.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","12:42:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62645",82052,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184395,-110.6843498,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916501558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33328.CHEM/results/916501558/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2021-10-21T10:57:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38272.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-09-22","11:58:00","MST",{"$nulls":4},41,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63108",82434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860056,-110.1179593,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943317975","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},41,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38272.CHEM/results/943317975/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-07-05T13:20:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34179.CHEM","Sample-Routine","Water","Groundwater","2021-11-05","09:51:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62780",82159,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2124082,-112.7552537,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-925210926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: R7.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34179.CHEM/results/925210926/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2021-12-28T10:27:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34984.CHEM","Sample-Routine","Water","Groundwater","2021-12-02","10:52:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62645",82052,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184395,-110.6843498,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994508152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34984.CHEM/results/994508152/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-02T11:38:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39579.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","10:00:00","MST",{"$nulls":4},39.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63083",82409,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860822,-110.1179399,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667107","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},39.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39579.CHEM/results/953667107/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-10-12T10:05:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41706.CHEM","Sample-Routine","Water","Groundwater","2022-11-15","02:20:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62645",82052,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184395,-110.6843498,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994681124","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41706.CHEM/results/994681124/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:19:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41503.CHEM","Sample-Routine","Water","Groundwater","2022-11-22","01:01:00","MST",{"$nulls":4},32.09,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63092",82418,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2861373,-110.1179947,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969238554","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},32.09,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41503.CHEM/results/969238554/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-03-03T09:05:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39581.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","10:45:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63104",82430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2858486,-110.1177657,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667255","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39581.CHEM/results/953667255/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-10-12T10:05:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39589.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","10:30:00","MST",{"$nulls":4},39,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63108",82434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860056,-110.1179593,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667847","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},39,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39589.CHEM/results/953667847/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-10-12T10:05:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44705.CHEM","Sample-Routine","Water","Groundwater","2022-09-30","10:00:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63530",82842,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152019,-110.1540564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994693771","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44705.CHEM/results/994693771/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:20:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41629.CHEM","Sample-Routine","Water","Groundwater","2022-11-30","02:35:00","MST",{"$nulls":4},70.74,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962654831","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},70.74,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41629.CHEM/results/962654831/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-01-06T10:30:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41510.CHEM","Sample-Routine","Water","Groundwater","2022-11-22","01:28:00","MST",{"$nulls":4},35.75,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63108",82434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860056,-110.1179593,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969239143","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},35.75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41510.CHEM/results/969239143/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-03-03T09:05:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41606.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","01:40:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62663",82070,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.212516,-112.7553511,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994678445","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41606.CHEM/results/994678445/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:19:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42952.CHEM","Sample-Routine","Water","Groundwater","2022-09-03","08:44:00","MST",{"$nulls":4},73,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63224",82542,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4961,-111.7143,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992930548","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,73,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42952.CHEM/results/992930548/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-11-09T09:39:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43130.CHEM","Sample-Routine","Water","Groundwater","2022-12-16","12:15:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63530",82842,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152019,-110.1540564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994687667","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43130.CHEM/results/994687667/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:20:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38453.CHEM","Sample-Routine","Water","Groundwater","2022-06-09","02:20:00","MST",{"$nulls":4},47,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63132",82452,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7400961,-112.009445,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943319829","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},47,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38453.CHEM/results/943319829/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-07-05T13:20:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41502.CHEM","Sample-Routine","Water","Groundwater","2022-11-22","01:58:00","MST",{"$nulls":4},19.85,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63104",82430,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2858486,-110.1177657,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969238474","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},19.85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41502.CHEM/results/969238474/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-03-03T09:05:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41608.CHEM","Sample-Routine","Water","Groundwater","2022-12-07","12:34:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62780",82159,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2124082,-112.7552537,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994678634","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41608.CHEM/results/994678634/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:19:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35684.CHEM","Sample-Routine","Water","Groundwater","2022-02-25","01:08:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62780",82159,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2124082,-112.7552537,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994636358","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35684.CHEM/results/994636358/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:15:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37050.CHEM","Sample-Routine","Water","Groundwater","2022-05-16","01:48:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63063",82397,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0480503,-112.1488712,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650908","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"TOTAL",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37050.CHEM/results/994650908/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:17:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37069.CHEM","Sample-Routine","Water","Groundwater","2022-05-10","11:31:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62780",82159,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2124082,-112.7552537,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994651375","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37069.CHEM/results/994651375/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:17:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40677.CHEM","Sample-Routine","Water","Groundwater","2022-05-10","03:12:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63530",82842,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152019,-110.1540564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994669026","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40677.CHEM/results/994669026/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:18:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40272.CHEM","Sample-Routine","Water","Groundwater","2022-09-23","05:40:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62780",82159,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2124082,-112.7552537,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956948469","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40272.CHEM/results/956948469/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-10-28T11:00:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39563.CHEM","Sample-Routine","Water","Groundwater","2022-09-14","10:16:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63132",82452,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7400961,-112.009445,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953579403","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39563.CHEM/results/953579403/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2022-10-07T10:34:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39295.CHEM","Sample-Routine","Water","Groundwater","2022-08-24","11:45:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62645",82052,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184395,-110.6843498,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994660387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39295.CHEM/results/994660387/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",null,"2023-12-04T10:17:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39480.CHEM","Sample-Routine","Water","Groundwater","2022-09-07","10:00:00","MST",{"$nulls":4},38.8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62867",82238,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529904,-110.0339711,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663425","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,38.8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39480.CHEM/results/994663425/resdetectqntlmts","Laboratory Reporting Level",40,"ug/L",null,"2023-12-04T10:18:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45166.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","04:13:00","MST",{"$nulls":4},39.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62873",82244,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529041,-110.0338758,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974992518","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,39.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45166.CHEM/results/974992518/resdetectqntlmts","Laboratory Reporting Level",40,"ug/L",null,"2023-05-25T10:52:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45172.CHEM","Sample-Routine","Water","Groundwater","2023-03-24","10:37:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62867",82238,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529904,-110.0339711,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974992872","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45172.CHEM/results/974992872/resdetectqntlmts","Laboratory Reporting Level",40,"ug/L",null,"2023-05-25T10:52:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45533.CHEM","Sample-Routine","Water","Groundwater","2023-05-04","09:27:00","MST",{"$nulls":4},31.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62864",82235,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560426,-110.0236335,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,31.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45533.CHEM/results/975083674/resdetectqntlmts","Laboratory Reporting Level",40,"ug/L",null,"2023-05-30T10:53:27","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150790-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","16:25:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79943","THOMPSON TDI-3",{"$nulls":4},34.9024417,-110.1635339,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552137726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150790-gwdb/results/552137726/resdetectqntlmts","Lower Reporting Limit",50,"ug/L",null,"2016-05-12T02:59:29","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150775-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","18:00:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79943","THOMPSON TDI-3",{"$nulls":4},34.9024417,-110.1635339,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552094946","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150775-gwdb/results/552094946/resdetectqntlmts","Lower Reporting Limit",50,"ug/L",null,"2016-05-12T02:40:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150794-gwdb","Sample-Routine","Water","Groundwater","2015-05-14","08:45:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79950","THOMPSON TDI-21",{"$nulls":4},34.90249,-110.1636969,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552063155","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-05-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150794-gwdb/results/552063155/resdetectqntlmts","Lower Reporting Limit",50,"ug/L",null,"2016-05-12T02:27:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43143.CHEM","Sample-Routine","Water","Groundwater","2022-11-03","09:30:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63061",82395,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483203,-112.1490083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994683359","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1.",null,21,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43143.CHEM/results/994683359/resdetectqntlmts","Laboratory Reporting Level",50,"ug/L",null,"2023-12-04T10:19:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43142.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-11-03","09:30:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63061",82395,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483203,-112.1490083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994683285","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1.",null,21,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43142.CHEM/results/994683285/resdetectqntlmts","Laboratory Reporting Level",50,"ug/L",null,"2023-12-04T10:19:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39479.CHEM","Sample-Routine","Water","Groundwater","2022-09-07","07:40:00","MST",{"$nulls":4},38.6,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62872",82243,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529809,-110.0338286,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663376","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,38.6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39479.CHEM/results/994663376/resdetectqntlmts","Laboratory Reporting Level",50,"ug/L",null,"2023-12-04T10:18:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38485.CHEM","Sample-Routine","Water","Groundwater","2022-06-06","05:04:00","MST",{"$nulls":4},14,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62866",82237,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530049,-110.0337858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994655959","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2.",null,14,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38485.CHEM/results/994655959/resdetectqntlmts","Laboratory Reporting Level",50,"ug/L",null,"2023-12-04T10:17:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39475.CHEM","Sample-Routine","Water","Groundwater","2022-09-06","02:46:00","MST",{"$nulls":4},41,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62873",82244,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529041,-110.0338758,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,41,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39475.CHEM/results/994663165/resdetectqntlmts","Laboratory Reporting Level",50,"ug/L",null,"2023-12-04T10:18:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36946.CHEM","Sample-Routine","Water","Groundwater","2022-05-09","02:25:00","MST",{"$nulls":4},159.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62817",82195,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651699,-112.4536728,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994648378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,159.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36946.CHEM/results/994648378/resdetectqntlmts","Laboratory Reporting Level",50,"ug/L",null,"2023-12-04T10:16:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30470.CHEM","Sample-Routine","Water","Groundwater","2021-01-20","03:23:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62640",82047,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186721,-110.6839328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-879851976","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30470.CHEM/results/879851976/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2021-03-05T16:20:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38266.CHEM","Sample-Routine","Water","Groundwater","2021-09-21","04:30:00","MST",{"$nulls":4},23.52,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63086",82412,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2858495,-110.117931,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943317531","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},23.52,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38266.CHEM/results/943317531/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2022-07-05T13:19:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51373.CHEM","Sample-Routine","Water","Groundwater","2021-12-30","11:35:00","MST",{"$nulls":4},31.3,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63106",82432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2859565,-110.1178806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-991216707","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31.3,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51373.CHEM/results/991216707/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-10-19T10:31:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33322.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","04:20:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62642",82049,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186834,-110.6842638,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916501006","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33322.CHEM/results/916501006/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2021-10-21T10:57:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34993.CHEM","Sample-Routine","Water","Groundwater","2021-12-02","04:33:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62640",82047,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186721,-110.6839328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994508520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34993.CHEM/results/994508520/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-12-02T11:38:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33326.CHEM","Sample-Routine","Water","Groundwater","2021-09-17","08:44:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62640",82047,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186721,-110.6839328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916501374","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33326.CHEM/results/916501374/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2021-10-21T10:57:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34995.CHEM","Sample-Routine","Water","Groundwater","2021-12-03","11:22:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62642",82049,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186834,-110.6842638,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994508612","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34995.CHEM/results/994508612/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-12-02T11:38:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39309.CHEM","Sample-Routine","Water","Groundwater","2022-08-25","01:42:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62642",82049,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186834,-110.6842638,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994661680","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39309.CHEM/results/994661680/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-12-04T10:17:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39577.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","11:45:00","MST",{"$nulls":4},37,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63106",82432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2859565,-110.1178806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953666959","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},37,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39577.CHEM/results/953666959/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2022-10-12T10:05:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39573.CHEM","Sample-Routine","Water","Groundwater","2022-09-14","10:50:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63123",82443,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7400311,-112.0094914,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953580147","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},45,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39573.CHEM/results/953580147/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2022-10-07T10:34:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38962.CHEM","Sample-Routine","Water","Groundwater","2022-04-01","09:25:00","MST",{"$nulls":4},97,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62940",82306,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834931,-110.7759672,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-950633850","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},97,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38962.CHEM/results/950633850/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2022-08-30T11:00:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41690.CHEM","Sample-Routine","Water","Groundwater","2022-11-16","01:39:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62640",82047,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186721,-110.6839328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679641","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41690.CHEM/results/994679641/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-12-04T10:19:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38449.CHEM","Sample-Routine","Water","Groundwater","2022-06-09","02:55:00","MST",{"$nulls":4},44,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63123",82443,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7400311,-112.0094914,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943319531","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: M1.",null,44,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38449.CHEM/results/943319531/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2022-07-05T13:20:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41685.CHEM","Sample-Routine","Water","Groundwater","2022-11-16","12:50:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62642",82049,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186834,-110.6842638,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679172","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41685.CHEM/results/994679172/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-12-04T10:19:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38953.CHEM","Sample-Routine","Water","Groundwater","2022-04-01","08:25:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-950633099","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38953.CHEM/results/950633099/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2022-08-30T11:00:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41687.CHEM","Sample-Routine","Water","Groundwater","2022-11-15","01:00:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62646",82053,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184087,-110.6844699,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679363","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41687.CHEM/results/994679363/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-12-04T10:19:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45325.CHEM","Sample-Routine","Water","Groundwater","2023-03-31","11:00:00","MST",{"$nulls":4},44.92,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63123",82443,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7400311,-112.0094914,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974803645","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},44.92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45325.CHEM/results/974803645/resdetectqntlmts","Laboratory Reporting Level",59.8,"ug/L",null,"2023-05-23T13:51:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35446.CHEM","Sample-Routine","Water","Groundwater","2021-09-28","01:00:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63064",82398,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0480947,-112.1489441,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933542688","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35446.CHEM/results/933542688/resdetectqntlmts","Laboratory Reporting Level",74.8,"ug/L",null,"2022-03-25T10:44:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35326.CHEM","Sample-Routine","Water","Groundwater","2021-12-07","01:36:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62988",82354,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.33581,-110.9417227,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994634043","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35326.CHEM/results/994634043/resdetectqntlmts","Laboratory Reporting Level",74.8,"ug/L",null,"2023-12-04T10:15:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35311.CHEM","Sample-Routine","Water","Groundwater","2021-09-28","12:16:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62988",82354,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.33581,-110.9417227,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-932819941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35311.CHEM/results/932819941/resdetectqntlmts","Laboratory Reporting Level",74.8,"ug/L",null,"2022-03-18T10:55:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41253.CHEM","Sample-Routine","Water","Groundwater","2022-06-02","12:48:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62993",82359,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357048,-110.9417694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994674658","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41253.CHEM/results/994674658/resdetectqntlmts","Laboratory Reporting Level",74.8,"ug/L",null,"2023-12-04T10:19:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41251.CHEM","Sample-Routine","Water","Groundwater","2022-06-02","01:56:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62988",82354,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.33581,-110.9417227,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994674508","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41251.CHEM/results/994674508/resdetectqntlmts","Laboratory Reporting Level",74.8,"ug/L",null,"2023-12-04T10:19:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35853.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","01:45:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62988",82354,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.33581,-110.9417227,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994641063","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35853.CHEM/results/994641063/resdetectqntlmts","Laboratory Reporting Level",74.8,"ug/L",null,"2023-12-04T10:16:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34765.CHEM","Sample-Routine","Water","Groundwater","2021-12-07","07:42:00","MST",{"$nulls":4},41,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62867",82238,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529904,-110.0339711,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626637","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,Q7,T4.",null,41,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34765.CHEM/results/994626637/resdetectqntlmts","Laboratory Reporting Level",80,"ug/L",null,"2023-12-04T10:14:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41123.CHEM","Sample-Routine","Water","Groundwater","2022-11-08","08:45:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62864",82235,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560426,-110.0236335,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994669382","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41123.CHEM/results/994669382/resdetectqntlmts","Laboratory Reporting Level",80,"ug/L",null,"2023-12-04T10:18:39","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150787-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","15:40:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79950","THOMPSON TDI-21",{"$nulls":4},34.90249,-110.1636969,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552164272","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150787-gwdb/results/552164272/resdetectqntlmts","Lower Reporting Limit",100,"ug/L",null,"2016-05-12T03:12:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34840.CHEM","Sample-Routine","Water","Groundwater","2021-12-21","01:26:00","MST",{"$nulls":4},70,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62901",82272,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.480657,-112.0125032,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994627480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,70,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34840.CHEM/results/994627480/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",null,"2023-12-04T10:14:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35770.CHEM","Sample-Routine","Water","Groundwater","2022-03-09","08:59:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62867",82238,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529904,-110.0339711,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994638474","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35770.CHEM/results/994638474/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",null,"2023-12-04T10:15:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38461.CHEM","Sample-Routine","Water","Groundwater","2022-06-09","09:42:00","MST",{"$nulls":4},29.6,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62858",82229,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560194,-110.0236635,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994654482","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2.",null,29.6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38461.CHEM/results/994654482/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",null,"2023-12-04T10:17:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49087.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","03:25:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49087.CHEM/results/994704928/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",null,"2023-12-04T10:21:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35325.CHEM","Sample-Routine","Water","Groundwater","2021-12-07","02:32:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62975",82341,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358512,-110.9417394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994633963","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35325.CHEM/results/994633963/resdetectqntlmts","Laboratory Reporting Level",149,"ug/L",null,"2023-12-04T10:15:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35307.CHEM","Sample-Routine","Water","Groundwater","2021-09-28","02:20:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62975",82341,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358512,-110.9417394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-932819641","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35307.CHEM/results/932819641/resdetectqntlmts","Laboratory Reporting Level",149,"ug/L",null,"2022-03-18T10:55:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41258.CHEM","Sample-Routine","Water","Groundwater","2022-06-02","03:13:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62975",82341,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358512,-110.9417394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994675040","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41258.CHEM/results/994675040/resdetectqntlmts","Laboratory Reporting Level",149,"ug/L",null,"2023-12-04T10:19:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35861.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","03:03:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62975",82341,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358512,-110.9417394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994641674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35861.CHEM/results/994641674/resdetectqntlmts","Laboratory Reporting Level",149,"ug/L",null,"2023-12-04T10:16:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33998.CHEM","Sample-Routine","Water","Groundwater","2021-09-30","01:49:00","MST",{"$nulls":4},70,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62901",82272,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.480657,-112.0125032,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919350603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2,.",null,70,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33998.CHEM/results/919350603/resdetectqntlmts","Laboratory Reporting Level",160,"ug/L",null,"2021-11-23T10:08:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45169.CHEM","Sample-Routine","Water","Groundwater","2023-03-24","09:47:00","MST",{"$nulls":4},38,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62869",82240,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530225,-110.0338642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974992693","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,38,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45169.CHEM/results/974992693/resdetectqntlmts","Laboratory Reporting Level",160,"ug/L",null,"2023-05-25T10:52:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49406.CHEM","Sample-Routine","Water","Groundwater","2023-06-15","10:45:00","MST",{"$nulls":4},40.1,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62873",82244,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529041,-110.0338758,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983676193","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2,.",null,40.1,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49406.CHEM/results/983676193/resdetectqntlmts","Laboratory Reporting Level",160,"ug/L",null,"2023-07-26T11:01:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49411.CHEM","Sample-Routine","Water","Groundwater","2023-06-15","10:05:00","MST",{"$nulls":4},39.9,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62872",82243,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529809,-110.0338286,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983676489","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,39.9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49411.CHEM/results/983676489/resdetectqntlmts","Laboratory Reporting Level",160,"ug/L",null,"2023-07-26T11:01:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39477.CHEM","Sample-Routine","Water","Groundwater","2022-09-06","01:44:00","MST",{"$nulls":4},38.2,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62865",82236,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530049,-110.0337858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663279","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2.",null,38.2,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39477.CHEM/results/994663279/resdetectqntlmts","Laboratory Reporting Level",200,"ug/L",null,"2023-12-04T10:18:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39478.CHEM","Sample-Routine","Water","Groundwater","2022-09-07","09:09:00","MST",{"$nulls":4},38.9,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62869",82240,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530225,-110.0338642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663332","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2.",null,38.9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39478.CHEM/results/994663332/resdetectqntlmts","Laboratory Reporting Level",250,"ug/L",null,"2023-12-04T10:18:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36510.CHEM","Sample-Routine","Water","Groundwater","2021-12-03","03:26:00","MST",{"$nulls":4},215.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62912",82282,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387948,-112.1870131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937426757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},215.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36510.CHEM/results/937426757/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2022-05-03T12:38:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36429.CHEM","Sample-Routine","Water","Groundwater","2021-12-17","10:15:00","MST",{"$nulls":4},77,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937421851","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},77,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36429.CHEM/results/937421851/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2022-05-03T12:36:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38267.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","12:43:00","MST",{"$nulls":4},39.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63106",82432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2859565,-110.1178806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943317605","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},39.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38267.CHEM/results/943317605/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2022-07-05T13:19:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35312.CHEM","Sample-Routine","Water","Groundwater","2021-09-28","03:38:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62979",82345,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357929,-110.9418056,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-932820016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35312.CHEM/results/932820016/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2022-03-18T10:55:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35331.CHEM","Sample-Routine","Water","Groundwater","2021-12-07","04:08:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62979",82345,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357929,-110.9418056,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994634349","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35331.CHEM/results/994634349/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2023-12-04T10:15:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36493.CHEM","Sample-Routine","Water","Groundwater","2021-08-25","02:15:00","MST",{"$nulls":4},215,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62912",82282,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387948,-112.1870131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937425499","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},215,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36493.CHEM/results/937425499/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2022-05-03T12:37:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39588.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","11:00:00","MST",{"$nulls":4},42,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63095",82421,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860355,-110.1180487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667773","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},42,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39588.CHEM/results/953667773/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2022-10-12T10:05:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41505.CHEM","Sample-Routine","Water","Groundwater","2022-11-22","02:25:00","MST",{"$nulls":4},38.76,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63095",82421,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860355,-110.1180487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969238725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},38.76,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41505.CHEM/results/969238725/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2023-03-03T09:05:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35858.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","04:42:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62979",82345,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357929,-110.9418056,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994641445","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35858.CHEM/results/994641445/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2023-12-04T10:16:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41261.CHEM","Sample-Routine","Water","Groundwater","2022-06-02","06:04:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62979",82345,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357929,-110.9418056,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994675273","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41261.CHEM/results/994675273/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2023-12-04T10:19:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45338.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","09:30:00","MST",{"$nulls":4},37.33,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63095",82421,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860355,-110.1180487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974804091","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":11},37.33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45338.CHEM/results/974804091/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",null,"2023-05-23T13:51:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35768.CHEM","Sample-Routine","Water","Groundwater","2022-03-09","09:58:00","MST",{"$nulls":4},39.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62869",82240,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530225,-110.0338642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994638346","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,39.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35768.CHEM/results/994638346/resdetectqntlmts","Laboratory Reporting Level",320,"ug/L",null,"2023-12-04T10:15:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35268.CHEM","Sample-Routine","Water","Groundwater","2022-02-08","01:52:00","MST",{"$nulls":4},160,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62817",82195,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651699,-112.4536728,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994633067","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: Q2,T4,D2.",null,160,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35268.CHEM/results/994633067/resdetectqntlmts","Laboratory Reporting Level",320,"ug/L",null,"2023-12-04T10:15:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49408.CHEM","Sample-Routine","Water","Groundwater","2023-06-15","09:18:00","MST",{"$nulls":4},41,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62869",82240,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530225,-110.0338642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983676312","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2,.",null,41,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49408.CHEM/results/983676312/resdetectqntlmts","Laboratory Reporting Level",320,"ug/L",null,"2023-07-26T11:01:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45530.CHEM","Sample-Routine","Water","Groundwater","2023-05-04","08:55:00","MST",{"$nulls":4},31.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62858",82229,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560194,-110.0236635,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083510","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,31.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45530.CHEM/results/975083510/resdetectqntlmts","Laboratory Reporting Level",320,"ug/L",null,"2023-05-30T10:53:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33131.CHEM","Sample-Routine","Water","Groundwater","2021-09-07","03:50:00","MST",{"$nulls":4},43.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62869",82240,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530225,-110.0338642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916463001","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,D2,.",null,43.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33131.CHEM/results/916463001/resdetectqntlmts","Laboratory Reporting Level",400,"ug/L",null,"2021-10-19T11:13:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32932.CHEM","Sample-Routine","Water","Groundwater","2021-08-09","03:55:00","MST",{"$nulls":4},159.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62817",82195,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651699,-112.4536728,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-914941366","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2.",null,159.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32932.CHEM/results/914941366/resdetectqntlmts","Laboratory Reporting Level",400,"ug/L",null,"2021-10-01T11:40:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49409.CHEM","Sample-Routine","Water","Groundwater","2023-06-15","08:36:00","MST",{"$nulls":4},40.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62867",82238,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529904,-110.0339711,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983676370","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,40.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49409.CHEM/results/983676370/resdetectqntlmts","Laboratory Reporting Level",400,"ug/L",null,"2023-07-26T11:01:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34834.CHEM","Sample-Routine","Water","Groundwater","2021-12-21","02:38:00","MST",{"$nulls":4},70,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62899",82270,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4807826,-112.0124891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994627133","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,70,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34834.CHEM/results/994627133/resdetectqntlmts","Laboratory Reporting Level",500,"ug/L",null,"2023-12-04T10:14:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34831.CHEM","Sample-Routine","Water","Groundwater","2021-12-21","03:56:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62900",82271,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4806301,-112.0127084,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626956","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,72,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34831.CHEM/results/994626956/resdetectqntlmts","Laboratory Reporting Level",500,"ug/L",null,"2023-12-04T10:14:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34005.CHEM","Sample-Routine","Water","Groundwater","2021-09-30","03:38:00","MST",{"$nulls":4},72.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62900",82271,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4806301,-112.0127084,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919350985","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,72.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34005.CHEM/results/919350985/resdetectqntlmts","Laboratory Reporting Level",640,"ug/L",null,"2021-11-23T10:08:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34059.CHEM","Sample-Routine","Water","Groundwater","2021-11-09","02:22:00","MST",{"$nulls":4},160,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62817",82195,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651699,-112.4536728,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-921314814","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,160,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34059.CHEM/results/921314814/resdetectqntlmts","Laboratory Reporting Level",640,"ug/L",null,"2021-12-06T09:11:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34002.CHEM","Sample-Routine","Water","Groundwater","2021-09-30","02:45:00","MST",{"$nulls":4},74,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62899",82270,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4807826,-112.0124891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919350836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,74,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34002.CHEM/results/919350836/resdetectqntlmts","Laboratory Reporting Level",1000,"ug/L",null,"2021-11-23T10:08:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34764.CHEM","Sample-Routine","Water","Groundwater","2021-12-07","08:27:00","MST",{"$nulls":4},40.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62869",82240,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2530225,-110.0338642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994626573","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,Q7,T4.",null,40.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34764.CHEM/results/994626573/resdetectqntlmts","Laboratory Reporting Level",1300,"ug/L",null,"2023-12-04T10:14:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34837.CHEM","Sample-Routine","Water","Groundwater","2021-12-20","12:25:00","MST",{"$nulls":4},68,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-50963",61087,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.480339,-112.0131478,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994627309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4.",null,68,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34837.CHEM/results/994627309/resdetectqntlmts","Laboratory Reporting Level",2000,"ug/L",null,"2023-12-04T10:14:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34004.CHEM","Sample-Routine","Water","Groundwater","2021-09-29","03:59:00","MST",{"$nulls":4},68.2,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-50963",61087,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.480339,-112.0131478,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919901333","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":5},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: D2,T4,.",null,68.2,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34004.CHEM/results/919901333/resdetectqntlmts","Laboratory Reporting Level",2000,"ug/L",null,"2021-12-01T09:40:10","STORET"]
[]
[{"$nulls":42},"mean",{"$f":"AVERAGE(AR4693:AR5095)","v":2.5168539325842696},"ug/l"]
[{"$nulls":42},"median",{"$f":"MEDIAN(AR4693:AR5095)","v":2},"ug/l"]

{"sheet":"Ambient air","index":6,"n_rows":10210,"n_cols":83,"rows_kept":1125,"cut":true,"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
["OrganizationIdentifier","OrganizationFormalName","ActivityIdentifier","ActivityTypeCode","ActivityMediaName","ActivityMediaSubdivisionName","ActivityStartDate","ActivityStartTime/Time","ActivityStartTime/TimeZoneCode","ActivityEndDate","ActivityEndTime/Time","ActivityEndTime/TimeZoneCode","ActivityRelativeDepthName","ActivityDepthHeightMeasure/MeasureValue","ActivityDepthHeightMeasure/MeasureUnitCode","ActivityDepthAltitudeReferencePointText","ActivityTopDepthHeightMeasure/MeasureValue","ActivityTopDepthHeightMeasure/MeasureUnitCode","ActivityBottomDepthHeightMeasure/MeasureValue","ActivityBottomDepthHeightMeasure/MeasureUnitCode","ProjectIdentifier","ProjectName","ActivityConductingOrganizationText","MonitoringLocationIdentifier","MonitoringLocationName","ActivityCommentText","SampleAquifer","HydrologicCondition","HydrologicEvent","ActivityLocation/LatitudeMeasure","ActivityLocation/LongitudeMeasure","SampleCollectionMethod/MethodIdentifier","SampleCollectionMethod/MethodIdentifierContext","SampleCollectionMethod/MethodName","SampleCollectionMethod/MethodDescriptionText","SampleCollectionEquipmentName","ResultIdentifier","ResultDetectionConditionText","MethodSpeciationName","CharacteristicName","ResultSampleFractionText","ResultMeasureValue","ResultMeasure/MeasureUnitCode","MeasureQualifierCode","ResultStatusIdentifier","StatisticalBaseCode","ResultValueTypeName","ResultWeightBasisText","ResultTimeBasisText","ResultTemperatureBasisText","ResultParticleSizeBasisText","DataQuality/PrecisionValue","DataQuality/BiasValue","DataQuality/ConfidenceIntervalValue","DataQuality/UpperConfidenceLimitValue","DataQuality/LowerConfidenceLimitValue","ResultCommentText","USGSPCode","ResultDepthHeightMeasure/MeasureValue","ResultDepthHeightMeasure/MeasureUnitCode","ResultDepthAltitudeReferencePointText","SubjectTaxonomicName","SampleTissueAnatomyName","BinaryObjectFileName","BinaryObjectFileTypeCode","ResultFileUrl","ResultAnalyticalMethod/MethodIdentifier","ResultAnalyticalMethod/MethodIdentifierContext","ResultAnalyticalMethod/MethodName","ResultAnalyticalMethod/MethodUrl","ResultAnalyticalMethod/MethodDescriptionText","LaboratoryName","AnalysisStartDate","ResultLaboratoryCommentText","ResultDetectionQuantitationLimitUrl","DetectionQuantitationLimitTypeName","DetectionQuantitationLimitMeasure/MeasureValue","DetectionQuantitationLimitMeasure/MeasureUnitCode",null,null,"LabSamplePreparationUrl","LastUpdated","ProviderName"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303448","Sample-Routine","Water","Surface Water","2012-11-19","10:25:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05485605",null,"L-3250012 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 101000  per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OK","USGS Oklahoma Water Science Center","nwisok.01.01300353","Sample-Routine","Water","Surface Water","2012-11-28","11:37:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-07159735",null,"L-3340023 LC8285 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107222450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301736","Sample-Routine","Water","Surface Water","2012-12-05","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05373005",null,"L-3420030 X = LC8252 deleted per request from WSC Bode, PG, 12/7/12   Received December 06, 2012  Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235052","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300359","Sample-Routine","Water","Surface Water","2012-11-28","11:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01391100",null,"L-3340075 LC8252 deleted per Rose, paa, 11/29/12  Updated time from 1130 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01306829","Sample-Routine","Water","Surface Water","2012-12-11","12:40:00","MST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394847104570700",null,"L-3470006 Updated time from 1230 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107243373","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303140","Sample-Routine","Water","Surface Water","2012-12-04","12:10:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-08057410",null,"L-3400056 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301741","Sample-Routine","Water","Surface Water","2012-12-04","08:40:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05340041",null,"L-3400039 Updated time from 0830 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107235727","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01303146","Sample-Routine","Water","Surface Water","2012-11-19","13:40:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01421640",null,"L-3250019 LC8252 deleted per Rose, paa, 11/30/12  Updated time from 133000 per Romanok.  KB 05/13/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107213401","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-11-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01300361","Sample-Routine","Water","Surface Water","2012-12-10","12:10:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-01409480",null,"L-3460046 Updated time from 1200 per Romanok.  KB 05/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107068868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2012-12-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302227","Sample-Routine","Water","Groundwater","2013-09-12","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325858082480101",null,"L-2590039 X = PHARM is not a GCV, it's a PHARM   Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  FUS btl type, smpl sent to WHOI without ASR, ASR recvd 10/29/13, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305560","Sample-Routine","Water","Groundwater","2013-07-10","09:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-350206118082401",null,"L-1920075 X = DOC is not a GCC please correct your labels..  S2437 split to 20131920165, paa, 2/19/14",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94953318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301075","Sample-Routine","Water","Groundwater","2013-09-05","14:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345927078170301",null,"L-2490157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96380393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306346","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364300119400001",null,"L-2420367 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96373953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400096","Quality Control Sample-Field Replicate","Water","Groundwater","2013-12-10","11:00:00","CST",{"$nulls":13},"USGS - Minnesota Water Science Center","MN040-450655093244701",null,"L-3450050 Added agency code per Langer.  KB 02/13/14  Samples were received chilled at the WHOI lab.  Added agency code per Langer.  KB 8/13/14",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-97038996","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300295","Sample-Routine","Water","Groundwater","2013-09-12","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405817117425401",null,"L-2560044 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96537369","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300200","Sample-Routine","Water","Groundwater","2013-08-13","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333036081442108",null,"L-2270106 Received August 14, 2013  LC1792 corrected to Scgedule 1792, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1100..  time added to ASR per radon, paa, 8/15/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95650577","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300791","Sample-Routine","Water","Groundwater","2013-08-21","14:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382825075081601",null,"A-2350143 3 drops HCl in VOC's",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104233375","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300982","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",173,"feet",208,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-421600085350001",null,"L-2420481 Received August 31, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Updated agency code from 0 to USGS per Beeler.  KB 01/21/14","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96406756","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302622","Sample-Routine","Water","Groundwater","2013-08-28","11:20:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-412307091031601",null,"L-2410170 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96416767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01304485","Sample-Routine","Water","Groundwater","2013-08-27","12:00:00","MDT",{"$nulls":4},4.95,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-402104104404501",null,"A-2420473 3 drops HCl each for schedules 4436 and 4437","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96352943","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301151","Sample-Routine","Water","Groundwater","2013-09-10","16:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345941078105001",null,"L-2550057 1 bottle leaked, 1/4 sample missing, per TAL   ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96444849","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300810","Sample-Routine","Water","Groundwater","2013-08-26","13:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382403075233201",null,"L-2400035 Received August 27, 2013",null,"Not applicable","Routine sample",null,null,4044,"USGS parameter code 82398","Submersible jet pump",null,"Submersible positive-pressure pump","NWIS-96270095","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300818","Sample-Routine","Water","Groundwater","2013-08-28","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390505075353901",null,"A-2410207 2 drops HCl in VOCs",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104234663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306550","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420003",null,"L-2630079 Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.  X = Time on sample 1001. Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible positive-pressure pump","NWIS-96557211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306408","Sample-Routine","Water","Groundwater","2013-09-11","09:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364600119460002",null,"L-2590041 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96466782","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302189","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-314733085071401",null,"L-2690200 Radon LC1369 removed from this ASR by Login, customer should do the same, paa, 10/24/13  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96617213","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305583","Sample-Routine","Water","Groundwater","2013-07-18","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363645119420901",null,"L-2060065 X = 2 empty GCVs - logged from problem cooler,relabeled remaining GCVs,paa,7/25/13    Received July 19,2013..  S2437 split to 20132060192, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94984590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303635","Sample-Routine","Water","Groundwater","2013-08-21","12:50:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-440354088560701",null,"L-2380159 Received August 23,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113295181","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302557","Sample-Routine","Water","Groundwater","2013-08-19","12:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-420158093562001",null,"L-2380248 logged from problem cooler, GCVs and PHARM missing date and time, paa added, WSC notified, paa, 8/26/13  Samples were received chilled at the WHOI lab.  logged from problem cooler, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95679036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400463","Quality Control Sample-Field Replicate","Water","Groundwater","2013-12-12","10:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370500120250001",null,"L-3470071 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106778047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305546","Sample-Routine","Water","Groundwater","2013-07-08","12:50:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-381100121200501",null,"L-1900067 S2437 split to 20131900098, paa, 2/19/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94889338","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300162","Sample-Routine","Water","Groundwater","2013-05-06","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392726119460101",null,"L-1280032 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131280085, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94501761","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306400","Sample-Routine","Water","Groundwater","2013-09-10","10:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364316119360801",null,"L-2540014 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-112097888","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300815","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-382906075215101",null,"A-2400162 2 drops HCl in VOCs  Sample for Sch 1792",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96270551","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01300822","Sample-Routine","Water","Groundwater","2013-08-21","12:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420410111490401",null,"L-2350034 Received August 22, 2013    per Sue changed state and county codes  pwg  2013/09/16   Updated UC from UT per Masbruch.  KB 09/19/13..  Sta ID changed from 420410111490501 to 420410111490401 per Thiros, paa, 12/31/13  Samples were received chilled at the WHOI lab.   per Sue changed state an",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104187844","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301280","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303501087174801",null,"L-2610137 Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96718520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WV","USGS West Virginia Water Science Center","nwiswv.01.01300175","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393418078132201",null,"L-2330053 User Code VA changed to WV per A. Melberg, paa, 9/10/13  Begin date is missing in mandatory field, time = 1100, JNV  Samples were received chilled at the WHOI lab...  date added to ASR per NWQL ASRs, paa, 9/3/13..  User Code VA changed to WV per A. Melberg, paa, 9/10/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96337686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302223","Sample-Routine","Water","Groundwater","2013-09-16","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323842083393201",null,"L-2600160 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300051","Sample-Routine","Water","Groundwater","2013-06-25","14:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-343817079353709",null,"L-1770065 S2437 split to 20131770134, paa, 2/18/14  Corrected invalid LC1792 to Sch1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94764758","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300739","Sample-Routine","Water","Groundwater","2013-08-14","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390217076181401",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95458314","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300873","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","EDT",{"$nulls":6},"Below land-surface datum",270,"feet",280,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380147076351201",null,"L-2620149 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96501873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306542","Sample-Routine","Water","Groundwater","2013-09-18","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363700119590001",null,"L-2630166 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300196","Sample-Routine","Water","Groundwater","2013-08-28","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351113089513401",null,"A-2410226 2 drops HCl added to VOCs  Actual radon sample collection time: 1245 CDT (estimated + 30minutes) L-2410226 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96508627","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301210","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","CDT",{"$nulls":4},92,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-412538089215801",null,"L-2400205 Date & time added to ASR per btls, paa, 8/28/13  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96070182","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305615","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364356119374001",null,"L-2070169 PEST split to separate ASR @0931, paa 7/26/13  Received July 25, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95228768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306395","Sample-Routine","Water","Groundwater","2013-09-09","13:50:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364316119360101",null,"L-2540016 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96466310","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400292","Sample-Routine","Water","Groundwater","2013-12-03","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500119590001",null,"L-3380016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306537","Sample-Routine","Water","Groundwater","2013-09-16","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363100120050002",null,"L-2610093 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098446","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303380","Sample-Routine","Water","Groundwater","2013-07-31","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-453247088425701",null,"L-2130212 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113285583","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302857","Sample-Routine","Water","Groundwater","2013-09-03","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304603094101801",null,"L-2470133 Updated STAID from 304303094101701 as per Patty 10.23.14 MKS.  btl type is FUS, paa Samples were received chilled at the WHOI lab.  per Ging changed station id from 304303094101701   pwg  2013/09/07",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96436969","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301147","Sample-Routine","Water","Groundwater","2013-09-09","12:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345005078493601",null,"L-2550061 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300824","Sample-Routine","Water","Groundwater","2013-08-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-380022079025601",null,"L-2390043 Btl type for 2255 is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96294530","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305557","Sample-Routine","Water","Groundwater","2013-07-11","08:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-353833117424001",null,"L-1960027 Received Jul 12, 2013..  S2437 split to 20131960099, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94952873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302931","Sample-Routine","Water","Groundwater","2013-07-09","10:00:00","MDT",{"$nulls":4},21,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-410251102024201",null,"L-1930027 Received Jul 11, 2013..  S2437 split to 20131930237, paa, 2/20/14",null,"Not applicable","Routine sample",null,null,4080,"USGS parameter code 82398","Peristaltic pump",null,"Peristaltic pump","NWIS-94914690","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300321","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300719092294901",null,"L-2260165 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95515272","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300673","Sample-Routine","Water","Groundwater","2013-06-13","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",377,"feet",412,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312952089444201",null,"L-1650003 S2437 split to 20131650193, paa, 2/14/14  Field alk added per manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94718189","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302856","Sample-Routine","Water","Groundwater","2013-09-04","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305947093395001",null,"L-2480032 FA condition changed to improper preservation, JNV   Lab acidification lab code 3105 added, JNV   FA preserved by C.harris on 9/11/13 @ 10:38, JNV  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301259","Sample-Routine","Water","Groundwater","2013-09-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361224076514501",null,"L-2690094 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96580242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303070","Sample-Routine","Water","Groundwater","2013-09-12","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-281433097191300",null,"L-2560186 X = 1 4437 recvd broken GCV   Updated SID from 281418097193901 per Ging.  KB 8/5/14  ASRs recvd late & entered 1/21/14, paa   Updated SID from 281418097193901 per Ging.  KB 8/20/14  Updated SID from 281418097193901 per Ging.  KB 8/5/14  btl type is FUS, paa Samples were received chilled at",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96922915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300056","Sample-Routine","Water","Groundwater","2013-07-02","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352613088381501",null,"A-1860092 2 drops of HCl in VOCs  Actual radon collection time: 1325 L-1860092 S2437 split to 20131860105, paa, 2/19/14  Samples were received chilled at the WHOI lab.","McNairy Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95009041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306409","Sample-Routine","Water","Groundwater","2013-09-11","13:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364400119450002",null,"L-2590043 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-112098073","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01303480","Sample-Routine","Water","Groundwater","2013-07-30","11:30:00","MDT",{"$nulls":4},39,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-401544103443101",null,"A-2140130 5 drops HCl each for schedules 4436 and 4437","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95388806","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303412","Sample-Routine","Water","Groundwater","2013-08-14","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-433136089235301",null,"L-2270168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113289140","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300049","Sample-Routine","Water","Groundwater","2013-06-24","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-340823079514509",null,"L-1760159 S2437 split to 20131760221, paa, 2/18/14  Corrected invalid LC1792 to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94764296","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306341","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-29","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363700119550001",null,"L-2420364 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112097698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01301828","Sample-Routine","Water","Groundwater","2013-09-23","12:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392322094214601",null,"A-2670053 VOC's HAVE 3 DROPS HCL EACH VIAL  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres.  w/2mL NITRIC ACID <pH2  RADON SAMPL   (Mailed in Fed-Ex Box) alone   Sampled @ 1440",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96605644","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300438","Sample-Routine","Water","Groundwater","2013-08-28","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301312093094101",null,"L-2410172 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96361016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300729","Sample-Routine","Water","Groundwater","2013-07-23","08:30:00","CDT",{"$nulls":6},"Below land-surface datum",358,"feet",400,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-340658088425101",null,"L-2060078 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95323181","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300690","Sample-Routine","Water","Groundwater","2013-07-17","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-391832075560801",null,"L-2040031 Received July 19, 2013..  S2437 split to 20132040231, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94987707","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300106","Sample-Routine","Water","Groundwater","2013-08-07","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-331822081020809",null,"L-2210179 Received August 08, 2013  Corrected invalid LC1792 to schedule 1792, WSC emailed, paa, 8/26/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95412663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01400050","Sample-Routine","Water","Groundwater","2013-10-29","10:40:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-402504093364301",null,"A-3030141 VOC'S HAVE 3 DROPS HCL EACH VIAL  GW-RADCHEM--(6)- 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Box Alone)   Sampled @ 1240",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96766746","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300482","Sample-Routine","Water","Groundwater","2013-09-12","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303404091325402",null,"L-2560167 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96471666","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302623","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-293938095561301",null,"L-2190145 Sta ID corrected from 561400 to 561301 per Ging,paa,9/10/13  Missing fields mandatory for WHOI,paa Samples were received chilled at the WHOI lab.  X = Time not on RADON  Sta ID corrected from 561400 to 561301 per Ging,paa,9/10/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95466090","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300115","Sample-Routine","Water","Groundwater","2013-07-17","12:00:00","EDT",{"$nulls":4},490,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-360626083170401",null,"A-2000117 3 drops of HCL added to VOCs  Actual Radon Time: 1309 L-2000117 Received July 18, 2013..  S2437 split to 20132000305, paa, 3/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95443580","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300280","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394147119580801",null,"L-2380143 Received August 23,2013..  invalid med code GW corrected to WG, paa, 8/31/13  Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96429683","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300326","Sample-Routine","Water","Groundwater","2013-08-14","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-295446091403901",null,"L-2270150 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95516191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300789","Sample-Routine","Water","Groundwater","2013-08-19","11:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383056075500201",{"$nulls":3},"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95663386","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300911","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","CDT",{"$nulls":6},"Below land-surface datum",283,"feet",323,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334100088193001",null,"L-2420356 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96364177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306278","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","PDT",{"$nulls":4},96,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380204",null,"L-2340193 Received August 21, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96074450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400070","Sample-Routine","Water","Groundwater","2013-10-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335943085032801",null,"L-2970176 LC1369 deleted from this ASR, paa  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96755304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300276","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375224117145401",null,"L-2410074 Received August 28, 2013..  invalid med code GW corrected to WG, paa, 9/5/13  Received August 28, 2013  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96429232","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300944","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","EDT",{"$nulls":4},38,"feet",null,35,"feet",55,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-395259083561501",null,"L-2350169 Received August 22, 2013  Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96540973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300111","Sample-Routine","Water","Groundwater","2013-08-05","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311928085494201",null,"L-2180068 Samples were received chilled at the WHOI lab.","Tallahatta Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96823327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300224","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-15","09:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322025111033101",null,"L-1970157 S2437 split to 20131970172, paa, 3/13/14  Samples leaked a little cpm <20 7/16/13, TAL  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94987231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300979","Sample-Routine","Water","Groundwater","2013-08-27","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",53,"feet",83,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435200084280001",null,"L-2410118 Btl type is FUS, paa Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96406114","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300200","Sample-Routine","Water","Groundwater","2013-08-22","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350108089242401",null,"A-2380070 2 drops HCl added to VOCs L-2380070 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96510398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302194","Sample-Routine","Water","Groundwater","2013-09-23","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312235084095301",null,"L-2670020 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96631329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302183","Sample-Routine","Water","Groundwater","2013-08-29","18:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-314356084375901",null,"L-2420348 Received August 30, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96603610","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300058","Sample-Routine","Water","Groundwater","2013-06-25","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361802088194201",null,"A-1770042 H2S odor present     2 drops HCl in VOCs  H2S odor present     Actual sample collection time 1145 L-1770042 H2S odor present cmt added per Jim, paa, 6/26/13..  S2437 split to 20131770131, paa, 2/18/14  H2S odor present cmt added per Jim, paa, 6/26/13  Samples were received chilled at the W","McNairy Formation","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95009647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300140","Sample-Routine","Water","Groundwater","2013-08-20","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350253089323901",null,"L-2330060 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96423743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303373","Sample-Routine","Water","Groundwater","2013-07-23","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-461703088043901",null,"L-2060132 Received July 24, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113282579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305665","Sample-Routine","Water","Groundwater","2013-07-23","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364259119385402",null,"L-2060023 Received July 24, 2013..  GWMSA added to ASR for WSC,paa,8/2/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95324858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302626","Sample-Routine","Water","Groundwater","2013-08-21","10:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-431045095413901",null,"L-2350103 X = Sta id on sample 431118095401.  Updated station ID from 431118095413401 as per Shannon Stubbs, KMS11/07/2013  Samples were received chilled at the WHOI lab.  Updated station ID from 431118095413401 as per Shannon Stubbs, KMS11/07/2013  Updated SID from 431118095415401 per Stubbs.  KB 0",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96422865","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301069","Sample-Routine","Water","Groundwater","2013-08-29","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344323076451301",null,"L-2420331 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96378056","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300243","Sample-Routine","Water","Groundwater","2013-07-24","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305500091065201",null,"L-2070072 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95082355","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300150","Sample-Routine","Water","Groundwater","2013-07-31","12:00:00","EDT",{"$nulls":4},0,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351019084365501",null,"A-2130165 2 drops of HCL added to VOCs  Actual Radon time = 1325 L-2130165 Updated SID from 351002084372001 per Kingsbury.  KB 09/30/13  Samples were received chilled at the WHOI lab.  Updated SID from 351002084372001 per Kingsbury.  KB 09/30/13",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-96435297","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01400144","Sample-Routine","Water","Groundwater","2013-12-03","10:45:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384457091271701",null,"L-3390014 per Paul GWMSA added, pwg  Invalid NAWQA proposal corrected, paa Samples were received chilled at the WHOI lab.  X=1 GCV vial recvd empty    per Paul GWMSA added, pwg",null,"Not applicable","Not applicable",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-96973874","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300693","Sample-Routine","Water","Groundwater","2013-07-17","13:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-392359075370301",null,"L-2040030 Received July 19, 2013..  S2437 split to 20132040230, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94988152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301074","Sample-Routine","Water","Groundwater","2013-09-05","11:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345730078301702",null,"L-2490348 4436 vial 2 GCV not recvd, ASR time changed to match btls per Fitzgerald, paa, 9/6/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-11","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300118","Sample-Routine","Water","Groundwater","2013-08-21","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321505086104601",null,"L-2350054 Received August 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96911961","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302677","Sample-Routine","Water","Groundwater","2013-08-21","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303000095002001",null,"L-2350179 Received August 22, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = Date on sample 8/12/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95677221","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300163","Sample-Routine","Water","Groundwater","2013-09-11","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333924086352901",null,"L-2550119 verified HFL recvd, not indicated as shipped, paa, 9/24/13..  sta id changed to 333924086352701 per Gill, paa, 10/30/13  ASRs recvd late & entered 1/21/14, paa     corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab..  sta id changed to 333924086352","Fort Payne Chert/formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97173275","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300969","Sample-Routine","Water","Groundwater","2013-08-07","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345051078012103",null,"L-2240084 Received August 9, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95454344","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400243","Sample-Routine","Water","Groundwater","2013-11-20","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370200120280001",null,"L-3290106 X=a PEST is a PEST, not a GCV    Received November 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775206","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300788","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382439079344801",null,"L-2340310 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95670220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300708","Sample-Routine","Water","Groundwater","2013-07-24","12:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383231075383101",null,"L-2070134 Received July 25, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95056279","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300922","Sample-Routine","Water","Groundwater","2013-09-25","14:00:00","EDT",{"$nulls":4},259,"feet",null,575.5,"feet",796,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372148076461001",null,"L-2700161 Received September 26, 2013  ASR future smpl date of 20130928 corrected to match Radon as 20130925, paa, 9/30/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96616244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300108","Sample-Routine","Water","Groundwater","2013-08-06","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335103080230801",null,"L-2190076 Samples were received chilled at the WHOI lab.  Sch 1792, not LC, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95413151","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301856","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","EDT",{"$nulls":4},45,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310913084195301",null,"L-2190136 Updated time from 110000  per Buell.  KB 10/24/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95654715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302114","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-310552084435601",null,"L-2210148 Received August 08, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96549892","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305542","Sample-Routine","Water","Groundwater","2013-07-10","13:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365516120033401",null,"L-1930108 Received July 11, 2013..  S2437 split to 20131930245, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94887660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300090","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314647085333501",null,"L-2320155 Updated SID from 314658085331201 per Gill.  KB 4/11/14  One bottle did not list date & time per TALWA, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.     corrected station id per Gill   pwg  04/18/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96811163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303649","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452733089435101",null,"L-2550111 X = Time on DOC is 1201, the rest of the bottles have the correct time  ASRs recvd late & entered 1/21/14, paa  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113298638","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300832","Sample-Routine","Water","Groundwater","2013-08-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-374426079211101",null,"L-2400078 Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107025926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302915","Sample-Routine","Water","Groundwater","2013-09-09","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-260204097443701",null,"L-2530042 Updated STAID from 260212097444301 as per Patty 10.23.14 MKS.  ASRs recvd late & entered 1/21/14, paa. Updated STAID from 260212097444301 as per Patty 10.23.14 MKS.  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301260","Sample-Routine","Water","Groundwater","2013-09-24","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362244077015501",null,"L-2690096 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96580695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301389","Sample-Routine","Water","Groundwater","2013-09-16","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-440435091404901",null,"A-2600163 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6) - 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Exact Time: 1149  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2600163 Samples were received chilled at the W",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96491554","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300294","Sample-Routine","Water","Groundwater","2013-08-14","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312658109360401",null,"L-2270082 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95513823","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302651","Sample-Routine","Water","Groundwater","2013-09-16","10:45:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-412938092380601",null,"L-2610026 Received September 17, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96490482","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400291","Sample-Routine","Water","Groundwater","2013-12-03","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365100120060001",null,"L-3380013 X=a PEST is a PEST not a GCV. FA is not labeled with date/time and station id  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776092","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302966","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271843098401101",null,"L-2620041 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96495760","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300151","Sample-Routine","Water","Groundwater","2013-07-18","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310630085355601",null,"L-2000277 X = No station id on samples..  S2437 split to 20132000313, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = No station id on sample",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97057695","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305888","Sample-Routine","Water","Groundwater","2013-08-14","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372505",null,"L-2270202 FA btl condition changed to improper preservation, JNV   Lab acidification lab code 3105 added, JNV    FA preserved by C.Harris on 8/19/13 @ 1005, JNV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95540441","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303021","Sample-Routine","Water","Groundwater","2013-09-24","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292923095091601",null,"L-2690194 Received September 25, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96555387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300612","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","CDT",{"$nulls":4},23,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444747096272001",null,"L-2700146 X = Improper sample container for DOC btl w/teal cap    Received September 26, 2013..   invalid NAWQA proposal corrected to CL13NAWSD to complete log in of custom requests and bill properly,paa,10/22/13  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab.  P",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96726466","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301328","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-400021077303101",null,"L-2540079 ASRs recvd late & entered 1/21/14, paa  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  FED EX LATE DELIVERY",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96409324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303382","Sample-Routine","Water","Groundwater","2013-08-01","14:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-454258088411601",null,"L-2140187 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113286444","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303433","Sample-Routine","Water","Groundwater","2013-08-05","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-433215088010001",null,"L-2190094 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113292256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400071","Sample-Routine","Water","Groundwater","2013-11-04","14:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380139077212901",null,"L-3090023 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96837255","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303647","Sample-Routine","Water","Groundwater","2013-09-09","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-442100089030001",null,"L-2530033 X = RU, FU, FCC & DOC have no time on sample  ASRs recvd late & entered 1/21/14, paa  Sta id on btl different from ASR per WHOI, sta id on btl 44210008930001, paa, 10/25/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113298176","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-11","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301226","Sample-Routine","Water","Groundwater","2013-09-17","15:45:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353143076575701",null,"L-2630119 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110390359","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301225","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351119076404801",null,"L-2630111 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110389902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300220","Sample-Routine","Water","Groundwater","2013-06-27","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-321321110450101",null,"L-1790118 S2437 split to 20131790271, paa, 2/18/14  Bottles have sample time @ 11:30, per TAL, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1130",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94867231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301403","Sample-Routine","Water","Groundwater","2013-09-24","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-454805096280901",null,"A-2690071 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM-- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH 2  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1311  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-2690071 Received September 25, 2013  Sample",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96552179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300687","Sample-Routine","Water","Groundwater","2013-07-16","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384152075290401",null,"L-1990092 Received July 17, 2013..  S2437 split to 20131990205, paa, 3/14/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104083149","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300198","Sample-Routine","Water","Groundwater","2013-08-15","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-334021079501308",null,"L-2310081 S1792 not LC1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95650087","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300050","Sample-Routine","Water","Groundwater","2013-06-26","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-342455080045509",null,"L-1780152 S2437 split to 20131780189, paa, 2/18/14  Invalid LC1792 corrected to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94849214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305612","Sample-Routine","Water","Groundwater","2013-07-25","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364457119553501",null,"L-2100109 S2437 PEST split to separate ASR @1331, paa, 7/29/13    Received July 26, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95227473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01400375","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-13","10:00:00","CST",{"$nulls":4},268,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-293516098325501",null,"L-3180136 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible helical rotor pump","NWIS-96944992","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301271","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-402058076124101",null,"L-2390146 Samples were received chilled at the WHOI lab.  sta id corrected from 40305 to 40205 per Low, paa, 1/3/14",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96051022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301230","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343855078315701",null,"L-2680058 Received September 24, 2013  Samples were received chilled at the WHOI lab.  X = recvd without ASR Eric faxed",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96504664","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302221","Sample-Routine","Water","Groundwater","2013-09-17","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323336084050601",null,"L-2610069 X = A PHARM is not a GCV  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96701634","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01301819","Sample-Routine","Water","Groundwater","2013-09-30","10:20:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-402332091342901",null,"L-2970126 Login delayed due to gov shutdown, ok to log recvd 10/24 from Paul B., paa, 10/24/13   Received October 01, 2013  File recvd late from TAL, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96604163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300082","Sample-Routine","Water","Groundwater","2013-07-15","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-313139085402101",null,"L-1990008 X = Samples do not have station id    Received July 16, 2013..  S2437 split to 20131990194, paa, 3/13/14  Samples were received chilled at the WHOI lab.  X = Station id not on label","Providence Sand","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96795508","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301395","Sample-Routine","Water","Groundwater","2013-09-18","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-435217095063401",null,"A-2620087 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6) - 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1155  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2620087 Samples were received chilled at the",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96492675","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300133","Sample-Routine","Water","Groundwater","2013-08-12","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-322405087342601",null,"L-2250122 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96912544","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300324","Sample-Routine","Water","Groundwater","2013-08-27","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-353232114200501",null,"L-2400155 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96279525","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300919","Sample-Routine","Water","Groundwater","2013-09-26","10:00:00","EDT",{"$nulls":4},100,"feet",null,190,"feet",208,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372823076433601",null,"L-2950071 Login delayed due to gov shutdown, ok log per B.Lindsey, paa, 10/22/13    Received September 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible helical rotor pump","NWIS-96615768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300945","Sample-Routine","Water","Groundwater","2013-09-30","12:00:00","EDT",{"$nulls":4},315,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-381531076583001",null,"L-2950073 Login delayed due to gov shutdown,ok log per B. Lindsey,paa,10/22/13   Received October 1,2013  File recvd late from TAL, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96781492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302202","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321838084435101",null,"L-2660027 Received September 20, 2013  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96633103","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01400374","Sample-Routine","Water","Groundwater","2013-11-14","09:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292331098294501",null,"L-3220033 Received November 15, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-96944555","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300070","Sample-Routine","Water","Groundwater","2013-07-30","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322643087020001",null,"L-2130003 Updated SID from 322644087020201 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14","Coker Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96776124","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300431","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324858109510701",null,"L-2320058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97321453","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01303450","Sample-Routine","Water","Surface Water","2013-05-20","12:15:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05451210",null,"L-1410060 Evn. ASR & smpls changed to 1215 per K.Romanok, paa, 5/21/13..  LC8252 deleted per Rose, paa, 5/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107224928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300913","Sample-Routine","Water","Groundwater","2013-08-28","14:30:00","CDT",{"$nulls":6},"Below land-surface datum",2210,"feet",2280,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332240089033401",null,"L-2410237 Samples were received chilled at the WHOI lab.  X = Time on samples 1430..  time added to ASR per radon, paa, 9/5/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96364801","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01303486","Sample-Routine","Water","Groundwater","2013-07-31","11:40:00","MDT",{"$nulls":4},5.8,"feet",{"$nulls":7},"USGS - Colorado Water Science Center","USGS-402213104015501",null,"A-2140132 6 drops HCl each for schedules 4436 and 4437.","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95387948","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301149","Sample-Routine","Water","Groundwater","2013-09-10","10:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341758077480802",null,"L-2550063 X = No time on RU  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443932","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306349","Sample-Routine","Water","Groundwater","2013-08-27","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364400119450001",null,"L-2470093 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96371045","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303418","Sample-Routine","Water","Groundwater","2013-08-07","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444302089144401",null,"L-2210439 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113290029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301223","Sample-Routine","Water","Groundwater","2013-09-17","08:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350717077002001",null,"L-2630113 X = Date on samples 9-17-13  Updated date from 2013/09/13 per Pointer.  KB 12/16/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110388985","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306358","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363500120030001",null,"L-2410019 Received August 28, 2013  Samples were received chilled at the WHOI lab.  smdugan added, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96371910","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300174","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","CDT",{"$nulls":4},98,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350543089473901",null,"A-2270007 3 drops HCl added to VOCs L-2270007 Received August 14, 2013  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96464256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301348","Sample-Routine","Water","Groundwater","2013-09-12","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-463618094183101",null,"A-2560042 VOCs HAVE 5 DROPS HCL EACH VIAL   Pleas lab filter schedule 2434  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH 2   LC=1364, LC=2164, shipped in 2nd cooler  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Actual time = 1335  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96448793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303374","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-460308088130601",null,"L-2110172 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300582","Sample-Routine","Water","Groundwater","2013-06-05","11:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385009075444401",null,"L-1580144 Received June 6, 2013,  STA ID corrected to 385009075444401 per Bringman GB 9/3/13..  S2437 split to 20131580152, paa, 2/14/14  STA ID corrected to 385009075444401 per Bringman GB 9/3/13",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94559591","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303377","Sample-Routine","Water","Groundwater","2013-07-30","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-451854087545501",null,"L-2130206 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113284297","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306281","Sample-Routine","Water","Groundwater","2013-08-20","09:00:00","PDT",{"$nulls":4},148,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380203",null,"L-2340191 Received August 21, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96159326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400078","Sample-Routine","Water","Groundwater","2013-10-24","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345255085174201",null,"L-3010111 Received October 25, 2013..  LC1369 removed from this ASR, paa, 11/4/13  Btl type FUS, not GCC, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96763067","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300404","Sample-Routine","Water","Groundwater","2013-08-21","12:00:00","MST",{"$nulls":4},75,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325104109421001",null,"L-2350253 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96935655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400457","Sample-Routine","Water","Groundwater","2013-12-09","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700119470002",null,"L-3450047 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776976","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302563","Sample-Routine","Water","Groundwater","2013-08-13","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-421016092020201",null,"L-2260157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95679968","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305541","Sample-Routine","Water","Groundwater","2013-07-11","10:10:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365418120035101",null,"L-1970165 S2437 split to 20131970173, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94887240","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301224","Sample-Routine","Water","Groundwater","2013-09-17","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350513076501501",null,"L-2630121 One btl recvd without label per Testam, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110389445","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301269","Sample-Routine","Water","Groundwater","2013-09-24","16:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351731076514101",null,"L-2700088 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110393177","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301685","Sample-Routine","Water","Groundwater","2013-08-19","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414400112050001",null,"L-2330051 ASR missing med code and smpl type, WG/9 added per PEST ASR, paa, 8/29/13  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-95681871","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01302838","Sample-Routine","Water","Groundwater","2013-09-18","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-393922096114901",null,"L-2630162 X = 1 GCV has date 9/?/2013  Btl type for Sch2255 i FUS, paa Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97186914","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301207","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":4},17,"feet",null,20,"feet",28,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-411432088234001",null,"L-2390164 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95912157","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301861","Sample-Routine","Water","Groundwater","2013-08-08","12:30:00","EDT",{"$nulls":4},22,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-311015084511901",null,"A-2210433 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-95668982","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300052","Sample-Routine","Water","Groundwater","2013-07-10","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354601084084201",null,"A-1930090 3 drops HCL added to VOC's  Actual Sample Time = 13:03 L-1930090 Received July 11, 2013   X = Please do not use pencil on ASR..  S2437 split to 20131930241, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94977484","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300286","Sample-Routine","Water","Groundwater","2013-09-04","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393351116000101",null,"L-2490177 Corrected med code to WG, paa   Recvd 9/6/13  Recvd 9/6/13  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96467946","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400242","Sample-Routine","Water","Groundwater","2013-11-19","10:20:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370800120270001",null,"L-3240015 X=PEST is PEST not GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300433","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310305092101202",null,"L-2400177 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96360558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300064","Sample-Routine","Water","Groundwater","2013-07-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-332036079244009",null,"L-2000084 Received July 18, 2013..  S2437 split to 20132000304, paa, 3/14/14  Corrected LC1792 to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94954827","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400459","Sample-Routine","Water","Groundwater","2013-12-10","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370200119590001",null,"L-3450049 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300169","Sample-Routine","Water","Groundwater","2013-08-14","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335323088074301",null,"L-2270136 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97177368","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WV","USGS West Virginia Water Science Center","nwiswv.01.01300172","Sample-Routine","Water","Groundwater","2013-08-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392158077525301",null,"L-2320020 X = Samples have date 8-19-13   Begin date is missing in mandatory field, time = 1100, JNV..  date added to ASR per btls, paa, 8/26/13..  User Code VA changed to WV per A. Melberg, paa, 9/10/13  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  User Code VA changed to WV",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96337224","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306534","Sample-Routine","Water","Groundwater","2013-09-17","13:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420001",null,"L-2610074 Updated Project Chief from Sue Dugan as per Sue Dugan 11.7.13 MKS.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96538536","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301628","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401012111354801",null,"L-2270198 Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95475574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300238","Sample-Routine","Water","Groundwater","2013-07-23","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302602091002505",null,"L-2060069 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95081886","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303022","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-291949095024801",null,"L-2690191 Received September 25, 2013  Updated SID from 292037095010501 per Ging.  KB 8/5/14  FUS btl type, paa Samples were received chilled at the WHOI lab.  Received September 25, 2013   Updated SID from 292037095010501 per Ging.  KB 8/5/14  Updated SID from 292037095010501 per Ging.  KB 8/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921974","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305563","Sample-Routine","Water","Groundwater","2013-07-09","08:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-333700114340001",null,"L-1910081 S2437 split to 20131910107, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96048698","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302169","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320051084061401",null,"A-2270163 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96562950","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301263","Sample-Routine","Water","Groundwater","2013-09-25","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355840076571001",null,"L-2730028 Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96582061","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300942","Sample-Routine","Water","Groundwater","2013-08-14","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",177,"feet",197,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-403857082191101",null,"L-2270191 Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96559910","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303632","Sample-Routine","Water","Groundwater","2013-08-21","17:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-442008089135201",null,"L-2380161 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113294745","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400072","Sample-Routine","Water","Groundwater","2013-10-23","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-341529085071301",null,"L-2970178 LC1369 deleted from this ASR, paa  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96754845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300115","Sample-Routine","Water","Groundwater","2013-09-11","08:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333642086065001",null,"L-2550121 X  =Time on samples 0900..  verified HFL recvd, not indicated as shipped, paa, 9/12/13   Updated SID from 333642086065101 per Gill.  KB 4/11/14  ASRs recvd late & entered 1/21/14, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.     corre",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96888911","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303415","Sample-Routine","Water","Groundwater","2013-08-08","15:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435453089184701",null,"L-2210437 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113289584","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300114","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-315522087045901",null,"L-2330058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96889501","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300316","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354709115220001",null,"L-2680157 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96730762","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300326","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-353513114161701",null,"L-2410259 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96280146","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300336","Sample-Routine","Water","Groundwater","2013-09-04","09:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320138111165301",null,"L-2480050 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96400549","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300330","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345516114364901",null,"L-2420145 FED EX LATE DELIVERY  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96278913","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305216","Sample-Routine","Water","Groundwater","2013-06-10","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-372100118250001",null,"L-1620245 S2437 split to 20131620256, paa, 2/14/14  GWMSA added due to exception, paa, 6/13/13  Samples were received chilled at the WHOI lab.  D-R'd per Mullin, sample ruined at contract lab.  KB 10/29/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94737897","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305596","Sample-Routine","Water","Groundwater","2013-07-15","10:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-345006118125701",null,"L-1990052 Received July 16, 2013..  S2437 split to 20131990197, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95016292","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303376","Sample-Routine","Water","Groundwater","2013-07-25","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452121088541301",null,"L-2110168 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01400007","Sample-Routine","Water","Groundwater","2013-11-06","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375700114254801",null,"L-3110028 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96891758","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300910","Sample-Routine","Water","Groundwater","2013-09-23","14:00:00","EDT",{"$nulls":6},"Below land-surface datum",279,"feet",354,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-374550077300501",null,"L-2680054 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96614340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302212","Sample-Routine","Water","Groundwater","2013-09-17","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323316084140501",null,"L-2610067 X = PHARM is not a GCV  Btl type is FUS, ASR missing mandatory pH, paa, 10/28/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96701171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301404","Sample-Routine","Water","Groundwater","2013-09-26","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-454900094342101",null,"L-2730066 Received September 27, 2013  Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96552765","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303656","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-432700089440001",null,"L-2350223 X = Date on samples 8/21/2013   Updated date from 2013/08/22 per Manteufel.  KB 02/03/14  Samples were received chilled at the WHOI lab.  radon recvd without smpl info on cylinder or smpl, added label per ASR, WSC emailed, paa, 8/22/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113299165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301258","Sample-Routine","Water","Groundwater","2013-09-23","14:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354953076484101",null,"L-2690100 X = GCV vial recvd broken  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96579784","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301266","Sample-Routine","Water","Groundwater","2013-09-23","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352301077300701",null,"L-2700086 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110391808","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300955","Sample-Routine","Water","Groundwater","2013-07-09","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352832076470102",null,"L-1920048 RECEIVED JULY 10, 2013..  S2437 split to 20131920163, paa, 2/19/14    X = Please correct your btl labels for SCH 2437, pest & LC 9017 Pharm.  They are not GCV's   LC's not indicated as add or delete, LC's added.  CSH  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-103032770","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301790","Sample-Routine","Water","Groundwater","2013-09-11","08:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-394200111490001",null,"L-2550014 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96440191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300741","Sample-Routine","Water","Groundwater","2013-07-24","09:30:00","CDT",{"$nulls":6},"Below land-surface datum",832,"feet",863,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342409088520901",null,"L-2100009 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95379365","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305616","Sample-Routine","Water","Groundwater","2013-07-22","14:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363806119345301",null,"L-2050201 Received July 23, 2013..  S2437 split to 20132050229, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95229190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301148","Sample-Routine","Water","Groundwater","2013-09-09","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343726078360201",null,"L-2550065 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96443472","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301154","Sample-Routine","Water","Groundwater","2013-09-12","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352839077040701",null,"L-2560053 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110388041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300735","Sample-Routine","Water","Groundwater","2013-07-24","15:45:00","CDT",{"$nulls":6},"Below land-surface datum",1609,"feet",1689,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345216089400201",null,"L-2100003 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95378132","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306533","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-17","09:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364200119420002",null,"L-2610076 Samples were received chilled at the WHOI lab..  Sta ID changed to 364200119420002 per Dugan, paa, 3/21/14",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96538091","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300281","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-385738119433601",null,"L-2320053 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96428784","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300161","Sample-Routine","Water","Groundwater","2013-07-16","11:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312534085203401",null,"L-1990082 X = No station id on samples    Received July 17, 2013..  S2437 split to 20131990199, paa, 3/13/14  Updated SID from 312517085201801 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.     corrected station id per Gill   pwg  04/18/14  X = You need to put station id on yo",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97172773","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300285","Sample-Routine","Water","Groundwater","2013-09-03","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392933117061701",null,"L-2470086 invalid med code GW corrected to WG, WSC notified, paa, 9/7/13  no time on ASR, WHOI emailed for time on btl, paa, 10/28/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96467494","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300676","Sample-Routine","Water","Groundwater","2013-06-25","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",315,"feet",345,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311642090113601",null,"L-1780043 Received June 26, 2013..  S2437 split to 20131780187, paa, 2/18/14  Received June 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94780770","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301071","Sample-Routine","Water","Groundwater","2013-09-03","16:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344734077254601",null,"L-2490159 Radon recvd completely unlabeled, added label per ASR, WSC notified requesting verify, paa, 9/4/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96378578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300717","Sample-Routine","Water","Groundwater","2013-07-30","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-393254075531801",null,"L-2130017 Received July 31, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95321788","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305213","Sample-Routine","Water","Groundwater","2013-06-11","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-342953117173101",null,"L-1630037 S2437 split to 20131630117, paa, 2/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94738454","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300137","Sample-Routine","Water","Groundwater","2013-09-16","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-334821086090001",null,"L-2610031 X = Improper sample container for RU in 1L glass bottle  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96918391","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300292","Sample-Routine","Water","Groundwater","2013-08-15","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-314322110030901",null,"L-2280189 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95513204","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300118","Sample-Routine","Water","Groundwater","2013-07-18","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355047084082701",null,"A-2030048 Drops of HCl added to VOCs  Actual Radon Time: 1212 L-2030048 Received July 19, 2013..  S2437 split to 20132030166, paa, 3/17/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95444192","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300170","Sample-Routine","Water","Groundwater","2013-08-20","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350403089445201",null,"L-2330062 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96463385","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300894","Sample-Routine","Water","Groundwater","2013-09-16","11:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393241077434201",null,"L-2600149 Updated UC from PA per Dieter.  KB 11/18/13  2 caps broken, sample for alpha beta empty, per testam, paa  Updated UC from PA per Dieter.  KB 11/18/13  Samples were received chilled at the WHOI lab.  Updated UC from PA per Dieter.  KB 11/18/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Other","NWIS-96479376","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300141","Sample-Routine","Water","Groundwater","2013-05-01","14:45:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392927119475201",null,"L-1230039 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131230103, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94382991","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300674","Sample-Routine","Water","Groundwater","2013-06-19","11:15:00","CDT",{"$nulls":6},"Below land-surface datum",210,"feet",250,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315920089541701",null,"L-1710186 S2437 split to 20131710195, paa, 2/18/14  1369 is lab code, not schedule, paa  Chg'd to S1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94772526","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301167","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","CDT",{"$nulls":6},"Below land-surface datum",18,"feet",28,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-393232088221801",null,"L-2320066 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95545324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305682","Sample-Routine","Water","Groundwater","2013-07-30","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364639120065001",null,"L-2130124 S2437 deleted from this ASR, see 2nd ASR @1331 for PEST, paa, 8/10/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95371649","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300704","Sample-Routine","Water","Groundwater","2013-07-23","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-374755075371001",null,"L-2060179 Received July 24, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95055836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300425","Sample-Routine","Water","Groundwater","2013-09-05","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324937113304501",null,"L-2490270 X = Time on samples 1100  Samples were received chilled at the WHOI lab.  X = Time on sample 1100",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97320825","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300208","Sample-Routine","Water","Groundwater","2013-08-14","14:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350018089190701",null,"A-2270187 2 drops HCl added to VOCs L-2270187 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96511276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300206","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350625089554901",null,"A-2410042 2 drops HCl/VOC vial L-2410042 Received August 28, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96509517","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300145","Sample-Routine","Water","Groundwater","2013-04-29","11:15:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391126119423201",null,"L-1210155 Lab codes not indicated as add or delete, LC's added, JNV..  one GCV converted to PEST and added, prog code corrected to GWMSA WSC notified, paa, 5/2/13..  S2437 split to 20131210174, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94425121","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300204","Sample-Routine","Water","Groundwater","2013-09-11","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351231089392301",null,"A-2550041 2  drops HCl/VOC vial L-2550041 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96510832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01303023","Sample-Routine","Water","Groundwater","2013-09-23","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300932094005301",null,"L-2680148 Received September 24, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96555820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306553","Sample-Routine","Water","Groundwater","2013-09-24","11:30:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364100119440001",null,"L-2680178 Smpl type changed from 1 to 9 per Evans, paa, 9/25/13     DOC condition changed to improper preservation, JNV  Samples were received chilled at the WHOI lab.  WSC emailed regarding smpl type 1, paa   Changed smpl type to 9 per Dugan, paa, 10/31/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96576242","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305617","Sample-Routine","Water","Groundwater","2013-07-23","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363928119401701",null,"L-2070165 X = Station ID diff. on btls's 363928119401701  PEST split to separate ASR @ 1001, paa 7/26/13  Received July 25, 2013,  STAID changed to 363928119401701 per Bennett GB 9/3/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95232156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300785","Sample-Routine","Water","Groundwater","2013-08-15","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385634078261501",null,"L-2280112 Btl type is FUS, paa   Begin date is missing in mandatory field, time = 1100, JNV Samples were received chilled at the WHOI lab.  date added to ASR per NWQL ASR, paa, 9/7/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107025473","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302965","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271505098073401",null,"L-2660071 Received September 20, 2013  Updated SID per Ging. 8/5/14  FUS btl type,paa Samples were received chilled at the WHOI lab.  Sta ID changed to 271505098073401 per Ging, paa, 9/25/14  Updated SID per Ging. 8/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96921542","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306284","Sample-Routine","Water","Groundwater","2013-08-19","14:40:00","PDT",{"$nulls":4},105,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380202",null,"L-2380206 ASR sta id corrected to match btls & per Dugan and fields corrected too, paa, 8/26/13  Updated SID from 364258119380201 per Dugan.  KB 09/10/13  Lid was off of one bottle (alpha/beta) and entire volume was lost   Station id on bottle is: 364258119380202   ASR sta id corrected per Dugan",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96074884","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300221","Sample-Routine","Water","Groundwater","2013-07-10","11:15:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333051112082001",null,"L-1930036 Received Jul 11, 2013..  S2437 split to 20131930238, paa, 2/20/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94924871","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303378","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-30","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-454107088011001",null,"L-2130208 S2437 deleted from this ASR, see second @1331, paa, 8/10/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113284726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300348","Sample-Routine","Water","Groundwater","2013-08-19","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313610091504501",null,"L-2320151 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95555138","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300277","Sample-Routine","Water","Groundwater","2013-07-30","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-344152111592301",null,"L-2130032 Received July 31, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95389988","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302554","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-430449096061301",null,"L-2380244 logged from problem cooler, paa  Samples were received chilled at the WHOI lab.  logged from problem cooler, smpl information added to GCVs by paa, 8/26/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95678562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300088","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314038085365401",null,"L-2390168 X = Time on sample 1200",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96801601","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01301526","Sample-Routine","Water","Surface Water","2013-05-13","11:40:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-324305097101900",null,"L-1350041 Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300666","Sample-Routine","Water","Groundwater","2013-07-08","14:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-373330075494601",null,"L-1920036 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131920161, paa, 2/19/14",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94892623","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300167","Sample-Routine","Water","Groundwater","2013-07-24","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-321100086344501",null,"L-2070098 Received July 25, 2013..  PEST and S2437 split to second ASR @1130, Lab ID 20132070161, paa, 7/26/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97176757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300696","Sample-Routine","Water","Groundwater","2013-07-18","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385715075253001",null,"L-2030146 Received July 19, 2013..  S2437 split to 20132030167, paa, 3/17/14",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-94988597","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300331","Sample-Routine","Water","Groundwater","2013-08-15","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-312038092192601",null,"L-2280129 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95515726","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306344","Sample-Routine","Water","Groundwater","2013-08-28","13:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364100119450001",null,"L-2420373 Received August 30, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96373509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300053","Sample-Routine","Water","Groundwater","2013-07-15","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353857084511801",null,"A-1990033 3 drops HCl added to VOCs  Actual Radon Sample Time: 14:13 L-1990033 Received July 16, 2013..  S2437 split to 20131990196, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94978083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301372","Sample-Routine","Water","Surface Water","2013-03-12","15:20:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02281200",null,"L-0730004 Updated time from 1500 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107230079","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-03-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302859","Sample-Routine","Water","Groundwater","2013-08-28","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-280951096593801",null,"L-2410129 FUS btl type, paa Samples were received chilled at the WHOI lab.  Lid was completely off one sample, but lost small amount of sample (aprox 150-175mLs) per Test Am, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368442","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PR","USGS Puerto Rico Water Science Center","nwispr.01.01301107","Sample-Routine","Water","Surface Water","2013-03-19","10:40:00","AST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-50055410",null,"L-0790103 Updated time from 103000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107219605","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-03","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302621","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-292944095550101",null,"L-2210241 Received August 08, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = Time of sample label 1006",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95465216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300086","Sample-Routine","Water","Groundwater","2013-07-08","12:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323528086205801",null,"L-1900068 S2437 split to 20131900099, paa, 2/19/14  Samples were received chilled at the WHOI lab.  X = Please put information on tube so that we do not have to open, PG","Coker Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96800988","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300297","Sample-Routine","Water","Groundwater","2013-09-10","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-404325116065801",null,"L-2540077 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300100","Sample-Routine","Water","Groundwater","2013-08-08","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355752082564201",null,"A-2210431 3 drops of HCL added to VOCs  Actual Radon time =  1334 L-2210431 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95426613","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300736","Sample-Routine","Water","Groundwater","2013-07-24","12:45:00","CDT",{"$nulls":6},"Below land-surface datum",492,"feet",552,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343706089111601",null,"L-2100006 Received July 25, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95378734","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302619","Sample-Routine","Water","Surface Water","2013-04-16","10:10:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-02335870",null,"L-1080111 Received April 17, 2013  Updated time from 100000 per Romanok.  KB 05/10/13  Deleted LC 8252 per Rose.  KB 05/30/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107221194","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300599","Sample-Routine","Water","Groundwater","2013-06-12","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-390126075575401",null,"L-1640024 S2437 split to 20131640198, paa, 2/14/14",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94621681","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305207","Sample-Routine","Water","Groundwater","2013-06-13","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-335700116300001",null,"L-1690057 X = 9017 PHARM & 2434 HFL are not GCV's    Received June 14, 2013..  S2437 split to 20131690165, paa, 2/18/14  Samples were received chilled at the WHOI lab.  Updated SID from 33570011630001 per Dugan.  KB 07/11/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95906708","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300153","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-16","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354041084243601",null,"A-1990083 3 drops of HCL added to VOCs  Radon actual time = 1244 L-1990083 X = Please do not use pencil on ASR   Received July 17, 2013  Samples were received chilled at the WHOI lab.  corrected eASR sta id for Creekside per G. Johnson,paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96436487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302165","Sample-Routine","Water","Groundwater","2013-08-13","12:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312346084520401",null,"L-2270074 Received August 14, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96562393","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400295","Sample-Routine","Water","Groundwater","2013-12-05","09:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370000120120001",null,"L-3400054 station id corrected per Sue D.  pwg 1/02/14  Samples were received chilled at the WHOI lab.   corrected station id per Sue D.  pg  5/5/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776798","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300202","Sample-Routine","Water","Groundwater","2013-09-12","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350327089421401",null,"A-2560154 2 drops HCl/VOC vial L-2560154 only 5 GCV vials recvd per Murtaugh, paa  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96509069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300668","Sample-Routine","Water","Groundwater","2013-07-10","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-380403075292901",null,"L-1960088 Received July 12, 2013..  S2437 split to 20131960102, paa, 2/20/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94893474","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300148","Sample-Routine","Water","Groundwater","2013-08-14","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350234089394504",null,"A-2270189 2 drops HCl added to VOCs L-2270189 Updated SID from 350235089394701 per Kingsbury.  KB 09/30/13  Samples were received chilled at the WHOI lab.  Updated SID from 350235089394701 per Kingsbury.  KB 09/30/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96425510","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302862","Sample-Routine","Water","Groundwater","2013-08-21","16:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301420095093201",null,"L-2350194 Received August 22, 2013    Per Ging changed station id from 301419095093301   pwg  2013/09/07  FUS btl type, paa Samples were received chilled at the WHOI lab.  Received August 22, 2013. Updated STAID from 301419095093301 as per Patty 10.23.14 MKS.  Updated STAID from 301419095093301 as p",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96369313","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301624","Sample-Routine","Water","Groundwater","2013-08-15","12:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401148112433002",null,"L-2310079 Samples were received chilled at the WHOI lab.","Valley Fill","Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible piston pump","NWIS-95475102","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300193","Sample-Routine","Water","Groundwater","2013-05-08","11:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391111119481901",null,"L-1340062 Received May 11, 2013..  S2437 split to 20131340161, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4060,"USGS parameter code 82398","Gas reciprocating pump",null,"Gas reciprocating pump","NWIS-94586331","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300270","Sample-Routine","Water","Groundwater","2013-08-06","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304612089512401",null,"L-2200021 Received August 7, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95430262","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300314","Sample-Routine","Water","Groundwater","2013-09-19","08:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405517114204101",null,"L-2630098 DOC condition changed to improper preservation, JNV  sta id correction per K. Thomas,paa,11/4/13  Samples were received chilled at the WHOI lab.  sta id correction per K. Thomas,paa,11/4/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96602216","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01400009","Sample-Routine","Water","Groundwater","2013-11-07","10:00:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361200115580001",null,"L-3120076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96939011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300198","Sample-Routine","Water","Groundwater","2013-09-10","13:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351528089350801",null,"A-2540036 2 drops HCl added to VOCs L-2540036 ASRs recvd late & entered 1/21/14, paa..  Sta ID changed to 351528089350801 per Kingsbury, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96509954","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303381","Sample-Routine","Water","Groundwater","2013-08-01","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-462416088191901",null,"L-2140189 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113286014","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305585","Sample-Routine","Water","Groundwater","2013-07-17","10:50:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363107119372201",null,"L-2000067 Received July 18, 2013..  S2437 split to 20132000302, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985015","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301228","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-18","12:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354552077382301",null,"L-2630064 Samples were received chilled at the WHOI lab.  corrected station id per WSC  pwg  1/30/814  smpl type 9 corrected to 7 per Erik, paa, 10/31/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96503748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300792","Sample-Routine","Water","Groundwater","2013-08-21","09:45:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384322075394401",null,"L-2350145 Received August 22, 2013",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104233803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301152","Sample-Routine","Water","Groundwater","2013-09-11","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343908078432003",null,"L-2550059 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96445309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302855","Sample-Routine","Water","Groundwater","2013-09-05","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-310935093352701",null,"L-2490137 FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96367572","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300428","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-314050091260501",null,"L-2380072 Received August 23, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96360106","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300985","Sample-Routine","Water","Groundwater","2013-08-29","09:00:00","EDT",{"$nulls":6},"Below land-surface datum",92,"feet",112,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-423200084490001",null,"L-2420479 Received August 31, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96407397","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301231","Sample-Routine","Water","Groundwater","2013-09-19","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342728077335701",null,"L-2680056 Received September 24, 2013  Samples were received chilled at the WHOI lab.  Updated SID from 342650077351501 per Pointer.  KB 01/10/14  X = Recvd without ASR Erik faxed corrected btl label per Brian, PG",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96505120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302620","Sample-Routine","Water","Groundwater","2013-08-08","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-290028095594700",null,"L-2210360 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.  X = 1 FA recvd  X = Time on sample 1032",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95464775","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300298","Sample-Routine","Water","Groundwater","2013-09-11","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-405030115500001",null,"L-2550083 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573942","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300300","Sample-Routine","Water","Groundwater","2013-08-06","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-312423110574901",null,"L-2190150 Updated SID from 312443110573001 per Beisner.  KB 01/02/14  Dropped and cracked lids on 2 bottles during receipt. Lost small amount of volume. Transferred to new containers per TALWA      Updated SID from 312443110573001 per Beisner.  KB 01/02/14  Samples were received chilled at the WHOI",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95530757","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305259","Sample-Routine","Water","Groundwater","2013-06-25","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-333130114394001",null,"L-1770062 DOC changed to improper preservation, paa..  GWMSA added, WSC to verify, paa, 6/29/13..  S2437 split to 20131770132, paa, 2/18/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125523816","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300149","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342640088065901",null,"L-1980064 X = No station id on samples..  S2437 split to 20131980174, paa, 3/13/14  Samples were received chilled at the WHOI lab.  X=Station ID not on label",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97057093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300723","Sample-Routine","Water","Groundwater","2013-07-11","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",1989,"feet",2074,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333618089074301",null,"L-1960028 Received Jul 12, 2013..  S2437 split to 20131960100, paa, 2/20/14  Received Jul 12,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95237689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305540","Sample-Routine","Water","Groundwater","2013-07-11","12:50:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365220120052601",null,"L-1970151 S2437 split to 20131970169, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94886821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301068","Sample-Routine","Water","Groundwater","2013-08-28","11:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344244077135801",null,"L-2420333 X = Only 2 GCVs for 4436 recvd  Few samples had loose lids and leaked. COCs were not in plastic bag and got soaked per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96377603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01400231","Sample-Routine","Water","Groundwater","2013-12-11","10:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302329087040001",null,"L-3460042 FUS btl typpe for S2255, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-97164340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301073","Sample-Routine","Water","Groundwater","2013-09-04","14:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351804077520101",null,"L-2490155 ASR missing mandatory pH & alk, paa Samples were received chilled at the WHOI lab.  Per Shanon F.  corrected station id.  pwg  1/13/2014",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300721","Sample-Routine","Water","Groundwater","2013-07-09","10:45:00","CDT",{"$nulls":6},"Below land-surface datum",1480,"feet",1546,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325846088340801",null,"L-1910088 S2437 split to 20131910109, paa, 2/19/14  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95236492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300988","Sample-Routine","Water","Groundwater","2013-09-03","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",93,"feet",113,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-424900083150001",null,"L-2480071 Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96408037","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300976","Sample-Routine","Water","Groundwater","2013-08-26","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",150,"feet",185.8,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-435000084510001",null,"L-2410124 Lab Codes not indicated as add or delete,lab codes added,AAN  Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Samples received 8/29/13 @ 1015 am, 45 minutes left to run 2hr alpha beta per Test Am, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96405475","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305897","Sample-Routine","Water","Groundwater","2013-08-13","13:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372501",null,"L-2260083 Corrected to GWMSA, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95531694","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300746","Sample-Routine","Water","Groundwater","2013-07-23","12:30:00","CDT",{"$nulls":6},"Below land-surface datum",1303,"feet",1383,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341359089062201",null,"L-2060081 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95380599","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400289","Sample-Routine","Water","Groundwater","2013-12-02","09:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365400120070001",null,"L-3380015 X=a PEST is a PEST, not a GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775737","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300135","Sample-Routine","Water","Groundwater","2013-08-15","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-332357087524301",null,"L-2280114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96913142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300219","Sample-Routine","Water","Groundwater","2013-07-01","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-325329112405301",null,"L-1840085 Received July 2,2013..  S2437 split to 20131840130, paa, 2/19/14  Released Gross alpha beta per Mullin.  KB 6/17/15  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94866626","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300916","Sample-Routine","Water","Groundwater","2013-09-25","10:00:00","EDT",{"$nulls":4},210,"feet",null,247,"feet",272,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372148076461002",null,"L-2700159 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96615293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300142","Sample-Routine","Water","Groundwater","2013-08-27","18:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350514089553700",null,"A-2410044 3 drops of HCl added to VOCs L-2410044 Received August 28, 2013  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96424178","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400018","Sample-Routine","Water","Groundwater","2013-10-28","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",477,"feet",538,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375541076514301",null,"L-3030063 Received October 29, 2013  Samples were received chilled at the WHOI lab.  sta id corrected to 4301 per A. Melberg, paa, 1/21/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96781964","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NE","USGS Nebraska Water Science Center","nwisne.01.01300271","Sample-Routine","Water","Surface Water","2013-06-10","10:10:00","CDT",{"$nulls":14},"USGS-06770195",null,"L-1640193 Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107097321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302645","Sample-Routine","Water","Groundwater","2013-09-18","10:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-415613094591201",null,"L-2620166 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96489562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301072","Sample-Routine","Water","Groundwater","2013-09-04","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344002077013201",null,"L-2490161 Samples were received chilled at the WHOI lab.  X = Date on sample 9/4/13..  ASR date corrected to match Radon, paa, 9/7/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96379036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300223","Sample-Routine","Water","Groundwater","2013-07-18","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-330135111231701",null,"L-2000244 S2437 split to 20132000307, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = Time on sample 1110",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-97152093","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305593","Sample-Routine","Water","Groundwater","2013-07-16","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-344400117200001",null,"L-1990012 Received July 17, 2013..  S2437 split to 20131990195, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95016762","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301270","Sample-Routine","Water","Groundwater","2013-09-26","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354245077311701",null,"L-2730032 Received September 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110393632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306539","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-364300119420001",null,"L-2610095 Missing alk, WSC emailed, 10/31/13, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400240","Sample-Routine","Water","Groundwater","2013-11-18","10:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370500120190001",null,"L-3240012 X=PEST is not GCV it is a PEST  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106774675","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305543","Sample-Routine","Water","Groundwater","2013-07-10","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-365700120063401",null,"L-1930105 Received July 11, 2013    Btl type for S2437 is PEST,  paa..  S2437 split to 20131930242, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94888080","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300155","Sample-Routine","Water","Groundwater","2013-08-07","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-315820087202001",null,"L-2210136 Updated SID from 315915087202301 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97167396","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300879","Sample-Routine","Water","Groundwater","2013-09-19","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",618,"feet",659,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-373759076345501",null,"L-2660019 Received September 20, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96502818","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302200","Sample-Routine","Water","Groundwater","2013-09-18","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320859085003701",null,"L-2620156 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96632654","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400076","Sample-Routine","Water","Groundwater","2013-10-29","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344855084461101",null,"L-3030172 LC1369 removed from this ASR, paa, 11/4/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96762615","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400074","Sample-Routine","Water","Groundwater","2013-11-05","10:00:00","EST",{"$nulls":4},307,"feet",null,850,"feet",985,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365751076363001",null,"L-3100037 Date on btls 11/5/13..  corrected ASR date to match per A. Melberg, paa, 1/21/14  WSC emailed to verify field alk, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab...  field alk updated to 419.5 per Teunis, WHOI updated, paa, 11/13/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96837725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400027","Sample-Routine","Water","Groundwater","2013-10-31","11:00:00","EDT",{"$nulls":6},"Below land-surface datum",215,"feet",316,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372105077113601",null,"L-3080057 Received November 1, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96783378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300066","Sample-Routine","Water","Groundwater","2013-07-10","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-320848080454301",null,"L-1920128 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131920167, paa, 2/19/14  1792 is schedule, not lab code, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94955751","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","improper preservationsample was dilutedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300613","Sample-Routine","Water","Groundwater","2013-09-24","10:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-445330097071801",null,"L-2700147 X= Improper sample container for DOC btl w/teal cap    Received September 26, 2013..   invalid NAWQA proposal corrected to CL13NAWSD to complete log in of custom requests and bill properly,paa,10/22/13  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab. Sam",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96727024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301171","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-21","11:00:00","CDT",{"$nulls":4},60,"feet",null,77,"feet",102,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-383932090012601",null,"L-2350123 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95555768","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300275","Sample-Routine","Water","Groundwater","2013-07-29","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-342557112041303",null,"L-2120035 PEST & Sch2437 split to second ASR, paa, 7/31/13   Time not on PHARM, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95389378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302198","Sample-Routine","Water","Groundwater","2013-09-24","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320348084132701",null,"L-2680108 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96632220","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300265","Sample-Routine","Water","Groundwater","2013-07-31","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-301407092104201",null,"L-2130178 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Grab sample","NWIS-95420211","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300068","Sample-Routine","Water","Groundwater","2013-07-16","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-333850079014308",null,"L-1990137 Received July 17, 2013     GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131990208, paa, 3/14/14  LC1792 corrected to Sch 1792, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94990374","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300296","Sample-Routine","Water","Groundwater","2013-07-16","09:45:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315010111000701",null,"L-1990053 Received July 17, 2013..  S2437 split to 20131990198, paa, 3/13/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-95529513","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302914","Sample-Routine","Water","Groundwater","2013-09-10","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-271315097473201",null,"L-2540057 1 cap broken, 3/4 sample missing per TAL   ASRs recvd late & entered 1/21/14, paa  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96454122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306555","Sample-Routine","Water","Groundwater","2013-09-25","13:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364306119364401",null,"L-2700140 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96575802","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303639","Sample-Routine","Water","Groundwater","2013-08-27","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-460000088235501",null,"L-2400181 Bottles have station id of 460000088265501, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113295868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01400074","Sample-Routine","Water","Groundwater","2013-10-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-343914085165901",null,"L-3010107 Received October 25, 2013..  LC1369 removed from this ASR, paa, 11/4/13  Btl type is FUS, not GCC, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96762152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300147","Sample-Routine","Water","Groundwater","2013-05-07","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-393023119513701",null,"L-1300100 Received May 09, 2013..  S2437 split to 20131300206, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94424715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300060","Sample-Routine","Water","Groundwater","2013-06-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-360010088252901",null,"A-1780184 2 drops HCl in VOCs  H2S in sample  Actual sample collection time 0945 L-1780184 S2437 split to 20131780191, paa, 2/18/14  Samples were received chilled at the WHOI lab.","McNairy Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95010258","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305656","Sample-Routine","Water","Groundwater","2013-07-25","11:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364338119354602",null,"L-2110122 Received July 26, 2013..  NAWQA program code GWMSA added to ASR,paa,8/9/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95325321","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300144","Sample-Routine","Water","Groundwater","2013-08-28","14:30:00","CDT",{"$nulls":4},76,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351111089512501",null,"A-2410228 2 drops HCl added to VOC  Actual radon collection time: 1631 CDT L-2410228 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96424621","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302858","Sample-Routine","Water","Groundwater","2013-08-29","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-290209096302701",null,"L-2420230 FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96369796","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300402","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-13","12:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-314204110224201",null,"L-2260076 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96937465","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301688","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414233112174501",null,"L-2340074 X = Time on samples 1300, 1 GCV broken in cooler during shipping    Received August 21, 2013  Samples were received chilled at the WHOI lab.  X = Time on sample 1300",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible positive-pressure pump","NWIS-95682330","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300190","Sample-Routine","Water","Groundwater","2013-08-07","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363025082070401",null,"A-2250034 3 drops of HCL added to VOCs, H2S positive sniff test  Actual Radon time = 1311  H2S detected L-2250034 Received August 9, 2013  Samples were received chilled at the WHOI lab.  Updated date from 2013/08/06 per Kingsbury.  KB 3/7/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96472864","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300084","Sample-Routine","Water","Groundwater","2013-07-17","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-311805085462401",null,"L-2000053 Received July 18, 2013..  S2437 split to 20132000301, paa, 3/14/14  Samples were received chilled at the WHOI lab.  X = You need station id on labels","Providence Sand","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96802205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400290","Sample-Routine","Water","Groundwater","2013-12-02","12:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365200119560001",null,"L-3380014 X=a PEST is a PEST, not a GCV  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106775915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306287","Sample-Routine","Water","Groundwater","2013-08-19","12:00:00","PDT",{"$nulls":4},70,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119380201",null,"L-2320034 One bottle has lid broken off, and all sample is missing  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96075341","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302045","Sample-Routine","Water","Surface Water","2013-07-23","09:10:00","EST",{"$nulls":14},"USGS-02350524",null,"L-2060191 Received July 24, 2013  Deleted LC 8252 per Rose.  KB 09/16/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107104896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300318","Sample-Routine","Water","Groundwater","2013-09-30","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-364912114041201",null,"L-2940041 Login delayed due to gov shutdown,ok log per Bexfield,paa,10/21/13    Received October 1,2013  File recvd late from TAL, paa  Login delayed due to gov shutdown, ok log per Bexfield, paa, 10/21/13    Received October 1, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96731658","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01301282","Sample-Routine","Water","Groundwater","2013-09-18","11:00:00","CDT",{"$nulls":4},320,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305708087091201",null,"L-2620069 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96718991","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300051","Sample-Routine","Water","Groundwater","2013-07-09","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351253085105801",null,"A-1910015 Actual Sample Time 13:30 L-1910015 S2437 split to 20131910104, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94976882","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300065","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-325447080383601",null,"L-1970152 Received July 12, 2013..  S2437 split to 20131970170, paa, 3/13/14  Samples were received chilled at the WHOI lab.  Schedule 1792, not LC, paa",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-94955288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305590","Sample-Routine","Water","Groundwater","2013-07-17","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-351556116404601",null,"L-1990171 S2437 split to 20131990210, paa, 3/14/14  1 bottle had no time, TAL  Only smpl identification on RADON is 0936, logged by paa from problem cooler, paa, 7/18/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95015806","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300734","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","CDT",{"$nulls":6},"Below land-surface datum",925,"feet",1025,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345021088572201",null,"L-2110047 Received July 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95377529","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KY","USGS Kentucky Water Science Center","nwisky.01.01300436","Sample-Routine","Water","Groundwater","2013-09-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365200088210001",null,"L-2620048 X = FCC has no time, a PHARM is not a GCV    per Angie changed station ID and name  pwg  2013/09/26..  Sta ID changed to 365200088210001 per A. Crain, paa, 2/7/14  Samples were received chilled at the WHOI lab.  Updated SID from 365147088205702 and added station name per Crain.  KB 01/07/1",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96970314","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300477","Sample-Routine","Water","Groundwater","2013-09-11","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-304921092402202",null,"L-2550097 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96471207","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301405","Sample-Routine","Water","Groundwater","2013-09-10","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",48,"feet",88,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-400026091242501",null,"L-2540101 ASRs recvd late & entered 1/21/14,paa  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96432919","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300956","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-24","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350012077131101",null,"L-2110205 Corrected ST to GWMSA, paa   Received July 27, 2013..  S2437 deleted from this ASR, invalid S2612 corrected to LC2612, paa, 8/9/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95362122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305613","Sample-Routine","Water","Groundwater","2013-07-25","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364312119592901",null,"L-2100107 S2437 & PEST split to separate ASR @1001, paa, 7/29/13    Received July 26, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95227896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305891","Sample-Routine","Water","Groundwater","2013-08-14","10:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364255119372504",null,"L-2270210 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95531246","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300722","Sample-Routine","Water","Groundwater","2013-07-10","10:50:00","CDT",{"$nulls":6},"Below land-surface datum",1135,"feet",1185,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-331358088350001",null,"L-1920073 S2437 split to 20131920164, paa, 2/19/14  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95237088","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MT","USGS Montana Water Science Center","nwismt.01.01301628","Sample-Routine","Water","Surface Water","2013-08-28","10:40:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05014300",null,"L-2410104 Deleted 8252 per Rose.  KB 11/21/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107100098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306428","Sample-Routine","Water","Groundwater","2013-09-12","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363500120000001",null,"L-2590046 Received September 13, 2013  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112098261","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305246","Sample-Routine","Water","Groundwater","2013-06-17","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-331211116185101",null,"L-1690111 X = btl type for Sch2437 is PEST, not GCV   Updated SID from 331200116180001 per Dugan.  KB 07/12/13  Sta id on btl 331200116180001 per WHOI, paa Samples were received chilled at the WHOI lab.  Updated SID from 331200116180001 per Dugan.  KB 07/12/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94758029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302483","Sample-Routine","Water","Groundwater","2013-06-26","15:15:00","MDT",{"$nulls":4},10,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-405159102444201",null,"L-1790275 S2437 split from 20131790260, paa, 2/18/14","Alluvium and Terrace Deposits","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94803537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302861","Sample-Routine","Water","Groundwater","2013-08-26","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-291639097093901",null,"L-2400044 Received August 27, 2013  FUS btl type, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96368873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300112","Sample-Routine","Water","Groundwater","2013-07-11","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352745084341201",null,"A-1970120 3 drops HCl in VOCs  Actual Sample Time = 13:08 L-1970120 X = Please do not use electrical tape on DOC sample    Received July 12, 2013  Updated SID from 352741084342001 and date from 20130712 per Kingsbury.  KB 3/7/14.. S2437 split to 20131970166, paa, 3/13/14  Samples were received chill",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96472245","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301866","Sample-Routine","Water","Groundwater","2013-08-12","18:00:00","EDT",{"$nulls":4},38,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-314858084194901",null,"A-2250046 Accompanying pesticide sample  RadChem Samples",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-95669666","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400293","Sample-Routine","Water","Groundwater","2013-12-04","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365500120110001",null,"L-3400053 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776452","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300913","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","EDT",{"$nulls":4},164,"feet",null,200,"feet",220,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-372454076512801",null,"L-2680168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96614817","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300248","Sample-Routine","Water","Groundwater","2013-07-24","15:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-303001090274201",null,"L-2070070 Received July 25, 2013  Samples were received chilled at the WHOI lab.  X = Time sensitive time 1545",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95082821","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301221","Sample-Routine","Water","Groundwater","2013-09-16","12:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345637076383501",null,"L-2630115 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96503293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01300967","Sample-Routine","Water","Groundwater","2013-08-07","16:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343308077484501",null,"L-2240086 Received August 9, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95453906","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302936","Quality Control Sample-Field Replicate","Water","Groundwater","2013-07-11","10:30:00","CDT",{"$nulls":4},11,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-410959100582401",null,"L-1930218 S2437 split to 20131930249, paa, 2/20/14",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94915432","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300669","Sample-Routine","Water","Groundwater","2013-07-10","14:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-380027075410802",null,"L-1960087 Received July 12, 2013..  S2437 split to 20131960101, paa, 2/20/14  Even though samples lids were taped, some still leaked. JB 7/12/13 < 20cpm, TAL",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94893899","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302913","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-275725097562701",null,"L-2550106 ASRs recvd late & entered 1/21/14, paa  btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96453689","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305582","Sample-Routine","Water","Groundwater","2013-07-18","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363726119465201",null,"L-2030161 Received July 19, 2013..  S2437 split to 20132030169, paa, 3/17/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94984167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306275","Sample-Routine","Water","Groundwater","2013-08-21","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363337120070001",null,"L-2340269 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96158873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305545","Sample-Routine","Water","Groundwater","2013-07-09","10:10:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-381031121123901",null,"L-1930106 Received July 11, 2013..  S2437 split to 20131930243, paa, 2/20/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94888921","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400294","Sample-Routine","Water","Groundwater","2013-12-04","12:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365900120040001",null,"L-3400052 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106776625","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300941","Sample-Routine","Water","Groundwater","2013-08-13","15:00:00","EDT",{"$nulls":6},"Below land-surface datum",52,"feet",67,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-394208082252201",null,"L-2270196 Samples were received chilled at the WHOI lab.","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96559417","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305586","Sample-Routine","Water","Groundwater","2013-07-16","14:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363317119490401",null,"L-1990088 Btl type for S2437 is PEST not GVPEST, paa    Received July 17, 2013..  S2437 split to 20131990201, paa, 3/13/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985439","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301265","Sample-Routine","Water","Groundwater","2013-08-21","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-401002078254801",null,"L-2340287 GWMSA added, btl types corrected, paa, 8/22/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Other","NWIS-95667915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300839","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-371444080012701",null,"L-2400080 Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96295016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301261","Sample-Routine","Water","Groundwater","2013-09-24","15:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361252077074501",null,"L-2690102 4 bottles show sample date as 9/24/13. 9-23 will be used, per TestAm, paa..  ASR date corrected from 20130923 to 20130924 per Pointer, paa, 2/10/14  Samples were received chilled at the WHOI lab.  X= Date on sample 9/24/13..  ASR date corrected from 20130923 to 20130924 per Pointer, paa, 2",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96581152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306352","Sample-Routine","Water","Groundwater","2013-08-27","09:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364600119460001",null,"L-2410021 Received August 28,2013  2 of the bottles did not have station id #, date or time, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96374398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305210","Sample-Routine","Water","Groundwater","2013-06-12","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-341643116243101",null,"L-1640078 S2437 split to 20131640200, paa, 2/14/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94737449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300328","Sample-Routine","Water","Groundwater","2013-08-26","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-335825112435301",null,"L-2390103 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96280759","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300218","Sample-Routine","Water","Groundwater","2013-07-02","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332149113124601",null,"L-1860005 Received July 03, 2013..  S2437 split to 20131860104, paa, 2/19/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-94866036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","sample was dilutedsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400021","Sample-Routine","Water","Groundwater","2013-10-29","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365649077233801",null,"L-3030199 Samples were received chilled at the WHOI lab..  WSC emailed for sample time, WHOI did not send btl label information, paa, 11/12/13..  time of 1200 added per Teunis, paa, 11/13/13",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96782434","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301262","Sample-Routine","Water","Groundwater","2013-09-25","10:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353749076333501",null,"L-2730030 Received September 27,2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96581607","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302676","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300413094402101",null,"L-2380135 Received August 23, 2013  Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95676793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301264","Sample-Routine","Water","Groundwater","2013-09-26","10:45:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353605077483901",null,"L-2730034 Received September 27, 2013",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96582515","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306541","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-18","08:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-363700119550002",null,"L-2630170 Mising alk, WSC emailed, paa, 10/31/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96539013","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301267","Sample-Routine","Water","Groundwater","2013-08-22","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395625077585901",null,"L-2350258 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95668381","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400081","Sample-Routine","Water","Groundwater","2013-11-07","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-364151076571701",null,"L-3160061 Received November 08, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96838196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301390","Sample-Routine","Water","Groundwater","2013-09-17","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-433617092494301",null,"A-2610085 VOCs HAVE 5 DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM--(6)- 1 LITER BOTTLES pres. w/2mL NITRIC ACID <pH2  RADON SAMPLE (Mailed in Fed-Ex Box) alone   Exact time: 1315  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-1314 L-2610085 Samples were received chilled at the WH",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96492016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SD","USGS South Dakota Water Science Center","nwissd.01.01300611","Sample-Routine","Water","Groundwater","2013-09-26","10:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-434704096440701",null,"L-2950077 Logged from problem cooler per Joyce,delay due to gov shutdown,paa,10/22/13  Logged from problem cooler per Joyce, delay due to gov shutdown, paa, 10/22/13  Proposal added, paa  Proposal corrected to CL13NAWSD, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96725909","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301268","Sample-Routine","Water","Groundwater","2013-09-24","12:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350420077084901",null,"L-2700188 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110392721","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306896","Quality Control Sample-Field Replicate","Water","Groundwater","2013-09-25","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351600116030002",null,"L-2700164 Received September 26, 2013   Updated SID from 351600116030001 per Vasquez.  KB 12/18/13  Samples were received chilled at the WHOI lab.   Updated SID from 351600116030001 per Vasquez.  KB 12/18/13  Updated SID from 351600116030001 per Vasquez.  KB 12/18/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-98339431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-19","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400024","Quality Control Sample-Field Replicate","Water","Groundwater","2013-10-30","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",264,"feet",420,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-370156077063801",null,"L-3040104 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96782906","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-08","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303430","Sample-Routine","Water","Groundwater","2013-08-12","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-431953088113701",null,"L-2250078 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113291811","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300819","Sample-Routine","Water","Groundwater","2013-08-28","13:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-391233075433102",null,"A-2410209 3 drops HCl in each VOC",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104235098","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300121","Sample-Routine","Water","Groundwater","2013-07-30","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352554084193001",null,"A-2130055 4 drops of HCL added to VOCs  Actual Radon time = 1426 L-2130055 Received July 31, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95444799","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301483","Sample-Routine","Water","Groundwater","2013-09-30","11:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-445132093392101",null,"A-2940037 VOCs HAVE 5 DROPS HCL EACH VIAL (please lab filter schedule 2434)  GW-RADCHEM -- (6) - 1 LITER BOTLLES pres w/2mL NITRIC ACID <pH2  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-14 L-2940037 Login delayed due to gov shutdown, ok log per Terrio, paa, 10/21/13   Per btl labels, lab filter a",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96578141","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-29","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306272","Sample-Routine","Water","Groundwater","2013-08-22","10:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363900119500001",null,"L-2350235 X = Time on Sample 1030",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112097516","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301259","Sample-Routine","Water","Groundwater","2013-08-15","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-403325077242001",null,"L-2280187 GWMSA added to ASR, paa  Sta id on btl 403325077342001 per WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95517179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300716","Sample-Routine","Water","Groundwater","2013-07-29","12:00:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-381754075083601",null,"L-2120071 Received July 30, 2013",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95321354","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300670","Sample-Routine","Water","Groundwater","2013-07-11","10:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-381245075404001",null,"L-1970136 Received July 12, 2013..  S2437 split to 20131970167, paa, 3/13/14",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94894327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301300","Sample-Routine","Water","Groundwater","2013-08-27","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-404510077093801",null,"L-2400098 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96162973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300279","Sample-Routine","Water","Groundwater","2013-07-31","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334657113365501",null,"L-2130098 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95390601","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01400078","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-06","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365147076343001",null,"L-3110102 STA ID changed per Alyssa M 11/26/13 GB  Samples were received chilled at the WHOI lab. STA ID changed per Alyssa M 11/26/13 GB",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96943034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301150","Sample-Routine","Water","Groundwater","2013-09-10","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342300077425401",null,"L-2550067 X = Date on bottles is 9-9-13  ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96444391","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01301340","Sample-Routine","Water","Groundwater","2013-09-11","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395804076084801",null,"L-2550048 ASRs recvd late & entered 1/21/14, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96431820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302648","Sample-Routine","Water","Groundwater","2013-09-17","10:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-414101094303802",null,"L-2610129 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96490010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300907","Sample-Routine","Water","Groundwater","2013-08-29","14:00:00","CDT",{"$nulls":6},"Below land-surface datum",1302,"feet",1368,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332056088420901",null,"L-2420353 Received August 30, 2013  Bottles are labeled 3/29/13 1400, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96362936","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303427","Sample-Routine","Water","Groundwater","2013-08-06","13:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-443810088311601",null,"L-2190092 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-113291366","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301787","Sample-Routine","Water","Groundwater","2013-09-09","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385752112225301",null,"L-2530044 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96439288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301265","Sample-Routine","Water","Groundwater","2013-09-23","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351806077434501",null,"L-2700084 Received September 26, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110391352","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300317","Sample-Routine","Water","Groundwater","2013-09-23","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361023115114401",null,"L-2670013 ASR time 0900 (corrected from 9000), paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96731214","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303371","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-440157089180501",null,"L-2060129 Received July 24, 2013..  PEST not recvd for this ASR, S2437 deleted, see 206-130 for pest, paa, 8/2/13  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113281717","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300821","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382843078363101",null,"L-2350198 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96294072","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-28","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300028","Sample-Routine","Water","Groundwater","2013-06-12","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302120087374201",null,"L-1650045 Received June 13, 2013..  S2437 split to 20131650195, paa, 2/14/14  Sample exceeds 72hrs per TAL, paa  Samples were received chilled at the WHOI lab.  X = Need to put label on outside of tube",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-94670165","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300917","Sample-Routine","Water","Groundwater","2013-08-15","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345740089141601",null,"L-2310001 Received August 16, 2013  Updated UC from TN per Kingsbury.  KB 09/11/13  Updated UC from TN per Kingsbury.  KB 09/11/13  WHOI recvd smpl without ASR originally, ASR recvd 11/8, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-96423304","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300727","Sample-Routine","Water","Groundwater","2013-07-22","15:45:00","CDT",{"$nulls":6},"Below land-surface datum",545,"feet",625,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-342111089124401",null,"L-2040214 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95312179","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400461","Sample-Routine","Water","Groundwater","2013-12-11","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370100120060001",null,"L-3470072 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301153","Sample-Routine","Water","Groundwater","2013-09-11","15:15:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-352200077230601",null,"L-2560051 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.  X = Time on sample 1315",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96445767","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300141","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332833086203001",null,"L-2540048 X = Date on samples 9/7/2013   Updated SID from 332849086203501 per Gill.  KB 4/11/14  Sample date on bottle says 9/17/13, per TAL    ASRs recvd late & entered 1/21/14, paa    corrected station id per Gill   pwg  04/18/14  Samples were received chilled at the WHOI lab.    corrected station",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96927678","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300298","Sample-Routine","Water","Groundwater","2013-07-23","09:15:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-330420112034301",null,"L-2060173 Received July 24,2013..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  Samples were received chilled at the WHOI lab.  medium code corrected from WS to WG per Beisner, paa, 8/26/13  medium code corrected from WS to WG per Beisner, paa, 8/26/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95530139","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300866","Sample-Routine","Water","Groundwater","2013-09-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-370328080263101",null,"L-2600138 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96481995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300725","Quality Control Sample-Field Replicate","Water","Groundwater","2013-08-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-383756078455601",null,"L-2320018 Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95514802","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305671","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364258119385601",null,"L-2050179 Received July 23, 2013..  GWMSA added, WSC to verify, paa, 8/2/13  GWMSA added to ASR, paa  Samples were received chilled at the WHOI lab...  sta id changed to 85601 per Dugan, paa, 10/30/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95327078","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300397","Sample-Routine","Water","Groundwater","2013-07-17","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332916110510201",null,"L-1990162 Updated SID from 332927110511701 per Beisner.  KB 12/13/13..  S2437 split to 20131990209, paa, 3/14/14  Samples were received chilled at the WHOI lab.  Updated SID from 332927110511701 per Beisner.  KB 12/13/13  Updated SID from 332927110511701 per Beisner.  KB 12/13/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96936255","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300067","Sample-Routine","Water","Groundwater","2013-07-09","14:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-324829079533000",null,"L-1910021 GCVs btl condition changed to improper preservation, JNV..  S2437 split to 20131910105, paa, 2/19/14  Corrected to schedule 1792, not lab code, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-94956213","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Container not preserved, Lab will run as is Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","improper preservationsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400245","Sample-Routine","Water","Groundwater","2013-11-21","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365900120140001",null,"L-3290104 X=a PEST is a PEST, not a GCV     Received November 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-106775562","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301174","Sample-Routine","Water","Groundwater","2013-08-22","11:00:00","CDT",{"$nulls":4},80,"feet",null,42,"feet",82,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375756088081201",null,"L-2380075 Received August 23, 2013  Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95671290","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305662","Sample-Routine","Water","Groundwater","2013-07-24","10:40:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-364259119385404",null,"L-2070171 GWMSA added to ASR, paa, 7/26/13   Received July 25, 2013  GWMSA added to ASR,paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-95326202","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303379","Sample-Routine","Water","Groundwater","2013-07-31","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-450755088125301",null,"L-2130210 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113285154","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303375","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-451805088363101",null,"L-2110170 Received July 26, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113283440","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300092","Sample-Routine","Water","Groundwater","2013-08-28","11:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-315244085100401",null,"L-2410140 Updated SID from 315241085100501 per Gill.  KB 4/11/14  Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/14  corrected station id per Gill   pwg  04/18/14","Tuscaloosa Group","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96811766","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300159","Sample-Routine","Water","Groundwater","2013-09-04","05:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324159087362001",null,"L-2480016 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-97173868","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300275","Sample-Routine","Water","Groundwater","2013-08-07","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302832090064101",null,"L-2210134 WHOI ASR missing alkalinity, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95430725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IA","USGS Iowa Water Science Center","nwisia.01.01302577","Sample-Routine","Water","Groundwater","2013-08-27","10:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-423846095141801",null,"L-2400168 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96069579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301229","Sample-Routine","Water","Groundwater","2013-09-19","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-354838076541201",null,"L-2630062 X = Time on samples 1000  Updated time from 100100 per Giorgino.  KB 8/5/15  Samples were received chilled at the WHOI lab.  X = Time on sample 1001",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96504205","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300277","Sample-Routine","Water","Groundwater","2013-08-26","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-381704117031401",null,"L-2400093 Received August 27, 2013..  invalid med code GW corrected to WG, paa, 9/5/13  Received August 27, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96427889","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300296","Sample-Routine","Water","Groundwater","2013-09-16","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-401115118301501",null,"L-2600153 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96573047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300242","Sample-Routine","Water","Groundwater","2013-07-09","10:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","AZ014-334638112314501",null,"L-1910086 Updated SID from 334639112314801per Partin.  KB 08/07/13..  S2437 split to 20131910108, paa, 2/19/14  Samples were received chilled at the WHOI lab.  Updated SID from 334639112314801per Partin.  KB 08/07/13  Updated SID from 334639112314801per Partin.  KB 08/07/13  X = Time not on sample",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95232791","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300400","Sample-Routine","Water","Groundwater","2013-07-25","09:30:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322549111191601",null,"L-2110058 Received July 26, 2013..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  Samples were received chilled at the WHOI lab..  medium code corrected from WS to WG per Beisner, paa, 8/26/13  medium code corrected from WS to WG per Beisner, paa, 8/26/13",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96936858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302225","Sample-Routine","Water","Groundwater","2013-09-16","10:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-324816083290901",null,"L-2600158 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96702509","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-ID","USGS Idaho Water Science Center","nwisid.01.01300594","Sample-Routine","Water","Surface Water","2013-06-18","12:10:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-13210360",null,"L-1710091 ID user code per Romanok, paa, 6/20/13  Deleted LC8252 per Rose.  KB 07/10/13",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107112487","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01301844","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-313415084475201",null,"L-2270076 Received August 14, 2013",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-95553116","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300790","Sample-Routine","Water","Groundwater","2013-08-20","09:15:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384630075524801",null,"A-2330078 1 drop HCl in VOC",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95663815","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300793","Sample-Routine","Water","Groundwater","2013-08-19","14:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-383100076061103",null,"L-2320038 S1792 unclear, paa, ok'd to TALWA",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95664244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300733","Sample-Routine","Water","Groundwater","2013-07-25","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",597,"feet",637,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-345002088374401",null,"L-2110051 Received July 26, 2013  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95376926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300217","Sample-Routine","Water","Groundwater","2013-06-26","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-321846110592801",null,"L-1790022 Received June 27, 2013..  S2437 split to 20131790270, paa, 2/18/14  GWMSA added per NWQL ASRs, paa  GWMSA added, WSC to verify, paa, 7/3/13 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-94846967","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301213","Sample-Routine","Water","Groundwater","2013-08-28","11:00:00","CDT",{"$nulls":4},134,"feet",null,135,"feet",150,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-422448088041901",null,"L-2410083 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-96272163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300100","Sample-Routine","Water","Groundwater","2013-07-09","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325627087043401",null,"L-1910053 X = Station ID not on btl's..  S2437 split to 20131910106, paa, 2/19/14  Samples were received chilled at the WHOI lab.  X = Station ID not on sample  Need label on outside of tube",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96813135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301067","Sample-Routine","Water","Groundwater","2013-08-28","09:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-343400077292201",null,"L-2420329 Few samples had loose lids and leaked. COCs were not in plastic bag - soaked!, per Test Am, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96377142","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302622","Sample-Routine","Water","Groundwater","2013-08-14","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-294040096542401",null,"L-2270120 Sta ID corrected from 542400 to 542401 per Ging,paa,9/10/13  Missing fields mandatory for WHOI,paa Samples were received chilled at the WHOI lab.  X = Only one FA bottle received  Sta ID corrected from 542400 to 542401 per Ging,paa,9/10/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95465651","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300127","Sample-Routine","Water","Groundwater","2013-07-23","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-361610083581801",null,"A-2060161 3 drops of HCL added to VOCs  Actual Radon time = 12:52 L-2060161 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104108276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01300421","Sample-Routine","Water","Groundwater","2013-08-05","10:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-331616111401101",null,"L-2180154 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-97270953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-09","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01300202","Sample-Routine","Water","Groundwater","2013-08-20","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-335128081250001",null,"L-2340223 Samples were received chilled at the WHOI lab.  Sch 1792 not LC1792, paa",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95651065","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01300991","Sample-Routine","Water","Groundwater","2013-09-04","13:00:00","EDT",{"$nulls":6},"Below land-surface datum",53,"feet",63,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-432500082320001",null,"L-2480069 Btl type is FUS, paa Samples were received chilled at the WHOI lab.  Out of 72hr time frame per TAL    ASRs recvd late & entered 1/21/14, paa","Outwash","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-96408673","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-07","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300054","Sample-Routine","Water","Groundwater","2013-06-27","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351004088351501",null,"A-1820069 3 drops HCI in VOC's  Actual Radon time = 1015 L-1820069 Received Jun 28, 2013.. S2437 split to 20131820140, paa, 2/19/14  Updated SID from 351008088350601 per Kingsbury.  KB 3/7/14  Samples were received chilled at the WHOI lab..  Sta ID changed to 351004088351501 per Kingsbury,paa,3/13/1","Eutaw Formation","Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-95010864","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-03","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400462","Sample-Routine","Water","Groundwater","2013-12-11","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700120090001",null,"L-3470073 Samples were received chilled at the WHOI lab..  sta id corrected from 9001 to 90001 per Dugan, paa, 2/10/14  Updated SID from 365700120090011 per Dugan.  KB 2/28/14  sta id corrected from 9001 to 90001 per Dugan, paa, 2/10/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106777863","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-12-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300668","Sample-Routine","Water","Groundwater","2013-05-30","11:15:00","CDT",{"$nulls":6},"Below land-surface datum",139,"feet",161,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-313400091210001",null,"L-1510001 S2437 split to 20131510155, paa, 2/14/14  Btl type for S2255 is FUS, paa Samples were received chilled at the WHOI lab.  Sample is outside 72hrs per TAL, paa..  corrected LC1792 to Schedule 1792,paa,7/6/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94695044","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302679","Sample-Routine","Water","Groundwater","2013-08-19","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302207096050600",null,"L-2320028 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95678095","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01300940","Sample-Routine","Water","Groundwater","2013-08-13","10:00:00","EDT",{"$nulls":6},"Below land-surface datum",65,"feet",90,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USEPA-394257082362603",null,"L-2270194 Samples were received chilled at the WHOI lab..  smpl date changed from 20130812 to 20130813 per Runkle, WHOI notified, paa, 10/28/13","Outwash","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96558923","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300311","Sample-Routine","Water","Groundwater","2013-08-20","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392212119223001",null,"L-2340238 Received August 21, 2013  Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Received August 21, 2013   Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Samples were received chilled at the WHOI lab.  Updated SID from 392300119213001 per Thomas.  KB 09/25/13  Updated SID",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-96574934","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300794","Sample-Routine","Water","Groundwater","2013-08-20","13:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-385023076013501",null,"A-2330080 3 drops HCl in VOC",null,"Stable, normal stage","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104234231","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-23","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300164","Sample-Routine","Water","Groundwater","2013-08-12","15:00:00","CDT",{"$nulls":4},60,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-350643089502001",null,"A-2320150 2 drops of HCl added to VOCs L-2320150 Recvd without ASR originally, paa    Recvd 8/14/13  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96462089","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01302678","Sample-Routine","Water","Groundwater","2013-08-20","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-302145095473901",null,"L-2340207 Missing fields mandatory for WHOI, paa Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95677660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300882","Sample-Routine","Water","Groundwater","2013-09-17","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-365525080564901",null,"L-2620055 btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96550326","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302209","Sample-Routine","Water","Groundwater","2013-09-17","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323255084141801",null,"L-2610071 X = A PHARM is not a GCV  Btl type is FUS, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96700736","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01306394","Sample-Routine","Water","Groundwater","2013-09-09","10:40:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-364316119360102",null,"L-2540012 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab..  NAWQA program code without NAWQA proposal, WSC emailed, paa, 10/29/13..  CL13NAWCA added per Dugan, paa, 11/15/13",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96465878","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301267","Sample-Routine","Water","Groundwater","2013-09-24","10:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-353257077285302",null,"L-2700186 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110392264","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01300809","Sample-Routine","Water","Groundwater","2013-08-26","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey","USGS-384606075115801",null,"L-2400038 Received August 27, 2013",null,"Stable, normal stage","Routine sample",null,null,4044,"USGS parameter code 82398","Submersible jet pump",null,"Submersible positive-pressure pump","NWIS-96269660","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-31","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300671","Sample-Routine","Water","Groundwater","2013-06-12","15:00:00","CDT",{"$nulls":6},"Below land-surface datum",650,"feet",700,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302825089042001",null,"L-1640162 Field alk added per Manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792, paa  S2437 split to 20131640201, paa, 2/14/14  verified PHARM not recvd for this ASR, LC9017 deleted, paa, 6/18/13",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94716983","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01301788","Sample-Routine","Water","Groundwater","2013-09-10","10:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373900113130001",null,"L-2540111 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.","Valley Fill","Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-96439732","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305584","Sample-Routine","Water","Groundwater","2013-07-17","14:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - California Water Science Center","USGS-363418119384201",null,"L-2000068 Received July 18, 2013..  S2437 split to 20132000303, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94986606","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01301168","Sample-Routine","Water","Groundwater","2013-08-20","11:00:00","CDT",{"$nulls":4},60,"feet",null,55,"feet",65,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-391127088273501",null,"L-2330040 Samples were received chilled at the WHOI lab.","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-95545955","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300670","Sample-Routine","Water","Groundwater","2013-06-12","10:00:00","CDT",{"$nulls":6},"Below land-surface datum",530,"feet",570,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310929088334101",null,"L-1650043 Received June 13, 2013    Lab codes not indicated as add or delete, LC's added, JNV  Field alk added per Manning, paa, 6/19/13 Samples were received chilled at the WHOI lab.  LC1792 corrected to S1792 per TALWA, time on btls is 10:00, paa    Updated time from 093500 per Manning.  KB 10/10/",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94716379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01301227","Sample-Routine","Water","Groundwater","2013-09-18","09:15:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-355220076371501",null,"L-2680110 X = Recvd without ASR logged in from problem cooler Sharon faxed 9/25/13, PG  ASR not recvd with smpls, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110390817","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01400087","Quality Control Sample-Field Replicate","Water","Groundwater","2013-11-20","11:00:00","CST",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-443306094125501",null,"L-3250095 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96957832","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-11-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01301347","Sample-Routine","Water","Groundwater","2013-09-11","12:00:00","CDT",{"$nulls":13},"USGS - Minnesota Water Science Center","USGS-465926093354201",null,"A-2550072 VOCs HAVE   DROPS HCL EACH VIAL   Please lab filter schedule 2434  GW-RADCHEM -- (6) - 1 LITER BOTTLES pres w/2mL NITRIC ACID <pH2 LC1505 and LC2170 were shipped in a 2nd cooler  RADON SAMPLE  (Mailed in Fed-Ex Box) alone   Exact Time: 1432  WOODS HOLE LAB   1 LITER CLEAR BOTTLE FOR C-13-1",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-96448332","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305587","Sample-Routine","Water","Groundwater","2013-07-16","12:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-363316119473001",null,"L-1990090 Received July 17, 2013..  S2437 split to 20131990203, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-94985858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300146","Sample-Routine","Water","Groundwater","2013-08-21","15:30:00","CDT",{"$nulls":4},71,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351448089421700",null,"A-2350039 2 drops HCl added to VOC L-2350039 Received August 22, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96425064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01300146","Sample-Routine","Water","Groundwater","2013-05-06","10:45:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392937119452601",null,"L-1280031 Lab codes not indicated as add or delete, LC's added, JNV..  S2437 split to 20131280084, paa, 12/23/13","Valley Fill","Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94424307","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-05-10","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303643","Sample-Routine","Water","Groundwater","2013-08-28","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-445647091215301",null,"L-2420148 Samples were received chilled at the WHOI lab.  Some samples had leaked. COC and cooler wet per Test Am, paa",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113297244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-01","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.01300102","Sample-Routine","Water","Groundwater","2013-07-22","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320431085315301",null,"L-2050150 X = Station id not on sample    Received July 23, 2013..  S2437 split to 20132050227, paa, 3/17/14   Updated SID from 320431085315401 per Gill.  KB 4/11/14  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.    corrected station id per Gill   pwg  04/18/","Eutaw Formation","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96813737","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01300178","Sample-Routine","Water","Groundwater","2013-09-10","08:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351315089310501",null,"A-2540042 2 drops HCl added to VOCs L-2540042 ASRs recvd late & entered 1/21/14, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-96461585","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-12","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.01300876","Sample-Routine","Water","Groundwater","2013-09-18","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-380103076315901",null,"L-2620114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96502347","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-09-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01300280","Sample-Routine","Water","Groundwater","2013-08-08","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",635,"feet",670,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-312144092401801",null,"L-2210320 Received August 09, 2013  WHOI ASR missing alkalinity, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-95431180","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-08-13","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01300743","Sample-Routine","Water","Groundwater","2013-07-23","16:15:00","CDT",{"$nulls":6},"Below land-surface datum",343,"feet",423,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-341519088393901",null,"L-2060085 Received July 24, 2013  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95379978","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01305610","Sample-Routine","Water","Groundwater","2013-07-16","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362921119335901",null,"L-1990089 Received July 17, 2013,  STA ID changed from 362621119335901 to 362921119335901 per Bennett GB..  S2437 split to 20131990202, paa, 3/14/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-95074449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CO","USGS Colorado Water Science Center","nwisco.01.01302479","Sample-Routine","Water","Groundwater","2013-06-24","14:20:00","MDT",{"$nulls":4},9.5,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-400237104500301",null,"L-1770009 LC not indicated as add or delete, LC added, JD..  S2437 split to 20131770130, paa, 2/18/14",null,"Not applicable","Routine sample",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-94804423","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-06-27","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01302191","Sample-Routine","Water","Groundwater","2013-09-25","13:30:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-312332084555101",null,"L-2690202 ASR missing mandatory alk, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-96617648","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-10-18","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01303372","Sample-Routine","Water","Groundwater","2013-07-23","09:30:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-461739087192201",null,"L-2060131 Received July 24, 2013  ASR missing field alk, WSC emailed, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113282145","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2013-07-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01402392","Sample-Routine","Water","Groundwater","2014-08-21","11:20:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-464418119432901",null,"L-2380179 Received August 22, 2014  Received August 22,2014",null,"Not applicable","Not applicable",null,null,4047,"USGS parameter code 82398","Submersible gear pump",null,"Submersible gear pump","NWIS-99204203","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400284","Sample-Routine","Water","Surface Water","2014-04-15","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214655255",null,"A-1070012 10 min time offset",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97702315","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400378","Sample-Routine","Water","Surface Water","2014-04-16","10:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0208524090",null,"A-1070135 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97747492","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401154","Sample-Routine","Water","Surface Water","2014-06-11","13:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02095181",null,"L-1690057 Received June17, 2014",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98459973","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401199","Sample-Routine","Water","Surface Water","2014-06-11","16:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0212430653",null,"L-1690092 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98477301","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401205","Sample-Routine","Water","Surface Water","2014-06-11","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0212467595",null,"A-1680169 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98478357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01402223","Sample-Routine","Water","Groundwater","2014-06-10","10:00:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-322018108392501",null,"L-1620192 S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98532731","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01400735","Sample-Routine","Water","Surface Water","2014-05-13","10:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02085500",null,"L-1360081 Received May 15, 2014..  ASR date changed from 20140512 to 20140513 per Cassy P,paa,6/6/14",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97955558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-16","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01400798","Sample-Routine","Water","Groundwater","2014-01-13","15:10:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380302121203201",null,"L-0150012 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-112099668","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-01-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404355","Sample-Routine","Water","Groundwater","2014-08-18","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361207121075501",null,"L-2330026 Received August 20, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-105560148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-22","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01400898","Sample-Routine","Water","Groundwater","2014-07-31","13:00:00","EST",{"$nulls":6},"Below land-surface datum",null,null,170,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-382556078565401",null,"L-2130077 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98823072","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-06","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MS","USGS Mississippi Water Science Center","nwisms.01.01400484","Sample-Routine","Water","Groundwater","2014-05-12","10:30:00","CDT",{"$nulls":6},"Below land-surface datum",1245,"feet",1325,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-323308090180901",null,"L-1330111 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-97966196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-15","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01402806","Sample-Routine","Water","Groundwater","2014-08-18","10:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-294345094364501",null,"L-2320022 Received August 19, 2014  S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab.  X=time on pest is 1400   Received August 19, 2014",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99090184","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401189","Sample-Routine","Water","Surface Water","2014-06-10","14:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-0214265808",null,"L-1690115 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98465895","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01403520","Sample-Routine","Water","Groundwater","2014-08-20","10:00:00","MDT",{"$nulls":13},"USGS - Colorado Water Science Center","USGS-365802105313101",null,"L-2340267 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-104282190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402295","Sample-Routine","Water","Groundwater","2014-07-15","11:00:00","CST",{"$nulls":4},230,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-441948088094901",null,"L-1970139 S1792 changed to S1979 by TAL, paa  Samples were received chilled at the WHOI lab.  X=no date on sample","Ordovician-Cambrian Systems","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-113366845","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-18","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01402046","Sample-Routine","Water","Surface Water","2014-06-11","09:10:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02207435",null,"A-1680209 4 Drops HCl",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98396156","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01500422","Sample-Routine","Water","Groundwater","2014-12-04","09:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361100119010001",null,"L-3390078 7th GCV is actually a PHARM,paa,12/5/14  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104659895","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-12-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404278","Sample-Routine","Water","Groundwater","2014-08-13","10:40:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363618121381901",null,"L-2300123 Received August 15, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-105558893","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MI","USGS Michigan Water Science Center","nwismi.01.01400502","Sample-Routine","Water","Groundwater","2014-08-18","09:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Michigan Water Science Center","USGS-461500085550001",null,"L-2320070 Received August 19, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Other","NWIS-98954097","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.01401127","Sample-Routine","Water","Groundwater","2014-08-26","13:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-392929077530202",null,"L-2400141 Received August 27,2014  Received August 27, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-99284451","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01401662","Sample-Routine","Water","Groundwater","2014-09-03","14:10:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-384902090451201",null,"A-2470115 Pest Sample  Environmental Sample: VOCs have 3 drops HCl in each vial  GW Radchem - (6) 1L bottles, preserved with 2mL NA  Radon sample collected @ 1505  University of Miami Tritium Laboratory  1 LITER BOTTLE FOR TRITIUM ANALYSIS",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Line-shaft turbine pump","NWIS-99209953","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-06","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402327","Sample-Routine","Water","Groundwater","2014-07-10","09:15:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-443921089152001",null,"L-1950012 Received July 11, 2014",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113370647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402933","Sample-Routine","Water","Groundwater","2014-05-15","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-332011116534301",null,"L-1390212 Received May 17, 2014  ASR missing mandatory field alk, paa   alk added per NWQL LC2109, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112106990","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28 The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-30","holding time exceededsee result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01401641","Sample-Routine","Water","Surface Water","2014-05-16","08:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02336120",null,"A-1400253 2002943  10 min offset",null,"Falling stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97962970","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-30","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404630","Sample-Routine","Water","Groundwater","2014-09-15","11:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-383916122473501",null,"L-2610121 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106888016","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-21","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01403521","Sample-Routine","Water","Groundwater","2014-08-27","11:00:00","MDT",{"$nulls":13},"USGS - Colorado Water Science Center","USGS-360027106063401",null,"L-2410097 Samples were received chilled at the WHOI lab.","Santa Fe Group","Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-99201965","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-04","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01400646","Sample-Routine","Water","Groundwater","2014-09-09","10:00:00","EST",{"$nulls":4},200,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-341249081320100",null,"L-2530014 proj acct chg per F.Falls, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-99256420","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-20","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401474","Sample-Routine","Water","Groundwater","2014-08-26","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-362336079270001",null,"L-2460143 Received August 29, 2014  Proposal corrected, paa Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-99190780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-09-05","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MA","USGS Massachusetts Water Science Center","nwisma.01.01401000","Sample-Routine","Water","Groundwater","2014-07-15","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-414859072185801",null,"L-1970078 ASR recvd from Miami lab 10/1/14, paa  Samples were received chilled at the WHOI lab.","Stratified Deposits, Undifferentiated","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98777022","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-17","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01401179","Sample-Routine","Water","Surface Water","2014-04-17","11:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,null,"USGS-02336410",null,"A-1120107 10 min time offset",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-97680305","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-04-25","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01402565","Sample-Routine","Water","Groundwater","2014-04-25","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-325122116562101",null,"L-1180173 RECEIVED APRIL 25, 2014  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112104378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-05-02","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01400468","Sample-Routine","Water","Groundwater","2014-07-21","12:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-321245091495501",null,"L-2030134 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-98765004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-24","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01404086","Sample-Routine","Water","Groundwater","2014-08-06","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700121580001",null,"A-2200034 DROPS OF VOC ACID= 3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106883755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-08-14","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NC","USGS North Carolina Water Science Center","nwisnc.01.01401183","Sample-Routine","Water","Surface Water","2014-06-11","08:50:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-02146470",null,"L-1690040 Received June17, 2014",null,"Stable, normal stage","Routine sample",null,null,70,"USGS parameter code 82398","Grab sample  (dip)",null,"Grab sample","NWIS-98464836","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-06-19","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.01400480","Sample-Routine","Water","Groundwater","2014-07-23","11:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-323308091310801",null,"L-2060048 S1792 changed to S1979 by TAL,paa  Samples were received chilled at the WHOI lab.  end date & time added per Roland, paa, 7/25/14",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-98765511","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-29","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01402598","Sample-Routine","Water","Groundwater","2014-07-22","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-444829089161301",null,"L-2050054 Received July 23, 2014",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-113377588","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2014-07-26","see result laboratory comment",null,"Estimated Detection Level",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01503555","Sample-Routine","Water","Groundwater","2015-07-16","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-314348094421401",null,"L-1980183 Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,8010,"USGS parameter code 82398","Other",null,"Other","NWIS-101354024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-07-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01501719","Quality Control Sample-Field Replicate","Water","Groundwater","2015-01-13","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361700119340001",null,"L-0140025 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112108390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-01-23","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01501441","Quality Control Sample-Field Replicate","Water","Groundwater","2015-05-14","11:05:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-382915100544201",null,"L-1350149 X=no station id on PHARM or PEST",null,"Stable, normal stage","Routine sample",null,null,8040,"USGS parameter code 82398","Spigot",null,"Jet pump","NWIS-100825791","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-21","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500742","Sample-Routine","Water","Groundwater","2015-04-16","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-292420081084001",null,"L-1100037 Received April 17, 2015  H2S - Yes Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-109648933","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-26","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01503101","Sample-Routine","Water","Groundwater","2015-09-02","16:10:00","PDT",{"$nulls":4},70.5,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-462824119140801",null,"L-2530076 FED EX LATE DELIVERY",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101838290","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-16","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500794","Sample-Routine","Water","Groundwater","2015-04-28","13:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-271752081214001",null,"L-1190110 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109653263","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600557","Quality Control Sample-Field Replicate","Water","Groundwater","2015-12-09","13:20:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390300121030001",null,"A-3450174 DROPS OF VOC ACID=5",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112116069","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503724","Quality Control Sample-Field Replicate","Water","Groundwater","2015-04-27","12:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-355447119250001",null,"A-1190049 DROPS OF VOC ACID = 3",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-104668921","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-02","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600018","Sample-Routine","Water","Groundwater","2015-10-07","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-410800122180001",null,"L-2860037 Received October 09, 2015  Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106933995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-10-17","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01504674","Sample-Routine","Water","Groundwater","2015-08-27","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-304246096521201",null,"L-2400164 Changed Station ID to current per P. Ging. JPC 8/29/16  Samples were received chilled at the WHOI lab. Changed Station ID to current per P. Ging. JPC 8/29/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-101831047","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600559","Sample-Routine","Water","Groundwater","2015-12-08","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391300120590001",null,"A-3430037 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112116437","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-11","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500792","Sample-Routine","Water","Groundwater","2015-04-23","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-264460080406001",null,"L-1170058 Received April 24, 2015  1792 switched to 1979 due to high solids  H2S =Yes 76ug/L Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-109652028","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503041","Sample-Routine","Water","Groundwater","2015-04-01","10:10:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361400119460001",null,"L-0920079 ASR missing WSC contact, paa  Samples were received chilled at the WHOI lab.  Smdugan added, S1792 changed to S1979 by ALS, paa",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-104666390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600595","Sample-Routine","Water","Groundwater","2015-12-17","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392400120570001",null,"A-3520032 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112117167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-28","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500783","Sample-Routine","Water","Groundwater","2015-08-11","16:00:00","CDT",{"$nulls":4},11.5,"feet",null,14.5,"feet",19.5,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-384646090375501",null,"A-2240121 Alternate contact-Kelly Warner(klwarner)/217-328-09727   drops HCL for VOC  Alternate contact - Kelly Warner, klwarner@usgs.gov 217-328-9725. Acidified with HNO3. Acidified with HNO3. RADCHEM - acidified HNO3","Quaternary System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-101521623","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-08-15","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01503313","Sample-Routine","Water","Groundwater","2015-04-09","10:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-354800119060001",null,"L-1000023 ASR missing WSC contact,paa  Samples were received chilled at the WHOI lab.  rhkent added, paa   1792 changed to 1679 due to re-prep required by low LCS--Recount outside holding time,per Mullin.  KB 6/30/15",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-104667466","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-04-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500568","Sample-Routine","Water","Surface Water","2015-06-22","13:30:00","CST",{"$nulls":13},"USGS - Illinois Water Science Center","USGS-05537000",null,"A-1770033 Attn: Mississippi River Study.",null,"Rising stage","Routine sample",null,null,15,"USGS parameter code 82398","10 or more equal width verticals, equal non-iso transit rate limited by velocity",null,"Weighted-bottle sampler","NWIS-101100449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01500976","Sample-Routine","Water","Groundwater","2015-06-29","12:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-301930082585001",null,"L-1810103 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109657592","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-07-04","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01505446","Sample-Routine","Water","Groundwater","2015-09-14","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373600121170001",null,"L-2600060 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106932931","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-24","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500975","Sample-Routine","Water","Surface Water","2015-08-26","13:00:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05543500",{"$nulls":3},"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-101745018","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-09-03","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.01500413","Sample-Routine","Water","Surface Water","2015-05-07","10:30:00","CST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-05541510",null,"L-1320087 X=no btl types on GCC, GCV, OXW, PEST, PHARM and TOC, no schedule or lab codes on btls   Received May 09, 2015..  Emailed WSC contact, missing proposal # for LC 9030,3406,9031,4440, & 8099, ACW, 5/13/15 Added proposal # CL15023, ACW, 5/19/15",null,"Stable, normal stage","Routine sample",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-100743136","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-14","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-SC","USGS South Carolina Water Science Center","nwissc.01.01500190","Sample-Routine","Water","Groundwater","2015-06-15","13:00:00","EST",{"$nulls":14},"USGS-324505081145100",null,"L-1670065 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8010,"USGS parameter code 82398","Other",null,"Line-shaft turbine pump","NWIS-101043504","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-06-20","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01501438","Sample-Routine","Water","Groundwater","2015-05-14","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-382915100544201",null,"L-1350064 Samples were received chilled at the WHOI lab.",null,"Stable, normal stage","Routine sample",null,null,8040,"USGS parameter code 82398","Spigot",null,"Jet pump","NWIS-100824600","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-16","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01600453","Sample-Routine","Water","Groundwater","2015-11-30","13:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-361801119380001",null,"A-3360131 DROPS OF VOC ACID =3",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106940150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-12-08","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01500568","Quality Control Sample-Field Replicate","Water","Groundwater","2015-05-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-425400070545401",null,"L-1400121 Added proposal number CL15NAWNH,and program/project code GWMSA per Flanagan,ACW,5/20/15  Samples were received chilled at the WHOI lab.","Bedrock","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-100718443","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2015-05-22","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601397","Sample-Routine","Water","Groundwater","2016-07-20","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-471928118412501",null,"L-2030129 X=no time on DOC & GCVs  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105284288","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WI","USGS Wisconsin Water Science Center","nwiswi.01.01603038","Sample-Routine","Water","Groundwater","2016-08-03","12:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431037090043401",null,"L-2439605 Samples were received chilled at the WHOI lab. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Submersible gear pump","NWIS-113537035","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701153","Sample-Routine","Water","Groundwater","2016-11-30","15:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-325527097305701",null,"L-3360010 Samples were received chilled at the WHOI lab.  Schedule 1792 changed to 1979 due to solids",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106530340","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01600678","Quality Control Sample-Field Replicate","Water","Groundwater","2016-05-23","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-425400070545401",null,"L-1450069 Samples were received chilled at the WHOI lab.","Bedrock","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103900426","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01700832","Sample-Routine","Water","Groundwater","2016-12-06","12:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365600118140001",null,"L-3440100 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-109454110","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01601988","Sample-Routine","Water","Groundwater","2016-01-26","12:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-282009099044001",null,"L-0270030 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103547870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-01-27","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01602333","Sample-Routine","Water","Groundwater","2016-03-15","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392800121150001",null,"L-0770037 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112122338","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-03-18","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01603730","Sample-Routine","Water","Groundwater","2016-06-16","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","TX001-352134101324007",null,"L-1690154 Changed Station ID to current per P. Ging. JPC 8/29/16  Samples were received chilled at the WHOI lab. Changed Station ID to current per P. Ging. JPC 8/29/16",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105054980","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NV","USGS Nevada Water Science Center","nwisnv.01.01600217","Sample-Routine","Water","Groundwater","2016-07-05","10:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392506119462201",null,"L-1890024 FED EX LATE DELIVERY  Samples were received chilled at the WHOI lab.",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105138590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01602049","Sample-Routine","Water","Groundwater","2016-02-09","15:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-285144097443401",null,"L-0410075 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103564480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-19","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01603740","Sample-Routine","Water","Groundwater","2016-05-25","13:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","TX001-341237102454818",null,"L-1470074 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105059384","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701155","Sample-Routine","Water","Groundwater","2016-11-28","12:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-320933099095201",null,"L-3340032 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106531590","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-11-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NM","USGS New Mexico Water Science Center","nwisnm.01.01604709","Sample-Routine","Water","Groundwater","2016-08-01","12:30:00","MDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351347106370301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-105514161","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01601401","Sample-Routine","Water","Groundwater","2016-01-14","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-281546099234601",null,"L-0150099 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-103269301","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-01-20","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01603924","Sample-Routine","Water","Groundwater","2016-05-16","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-351500118370001",null,"L-1410115 Time and date on RU & FU 1600  05102016  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108900390","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-25","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01603891","Sample-Routine","Water","Groundwater","2016-05-17","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371200119400001",null,"L-1440037 X=FU has an FA label. Ok to login warm per T.Mathany Chilled containers received warm at 18.6  Degrees C  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108898579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-25","sample was warm when receivedsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01604119","Sample-Routine","Water","Groundwater","2016-05-24","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392700120390001",null,"L-1470019 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112125494","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-05-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601368","Sample-Routine","Water","Groundwater","2016-06-28","11:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-464016119543901",null,"L-1820169 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105141450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01605762","Quality Control Sample-Field Replicate","Water","Groundwater","2016-08-08","09:50:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-391523120422401",null,"L-2240035 FED EX LATE DELIVERY  No tape, cap loose - no leak or loss of smaple Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-112127357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-08-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01601538","Sample-Routine","Water","Groundwater","2016-08-30","09:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-261537080141601",null,"L-2440030 Samples were received chilled at the WHOI lab. Result 77035, rejected on 12/21/21, because a national-scale QC evaluation for groundwater indicated that contamination bias likely resulted in relatively common detections taht do not represent environmental conditions.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109261196","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701147","Sample-Routine","Water","Groundwater","2016-12-12","12:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-333826097213601",null,"L-3480090 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106528456","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-12-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701159","Sample-Routine","Water","Groundwater","2016-11-16","10:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-300358099100901",null,"L-3220058 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106536719","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-11-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01606334","Sample-Routine","Water","Groundwater","2016-09-12","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384617120460001",null,"L-2590083 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112129960","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-09-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01601415","Sample-Routine","Water","Groundwater","2016-07-27","09:30:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-472756117373001",null,"L-2158705 Samples were received chilled at the WHOI lab.  Added user code WA. 8/4/2016 mec",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-105338489","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-WA","USGS Washington Water Science Center","nwiswa.01.01700212","Sample-Routine","Water","Groundwater","2016-11-16","12:30:00","PST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Washington Water Science Center","USGS-485930122431001",null,"L-3230003 X=received #1 of 4437 vials broken.  Added Schedules 4436 and 4437 per Huffman. 11/21/2016 mec  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"None","NWIS-106271902","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-11-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601613","Sample-Routine","Water","Groundwater","2016-02-02","09:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390500121000001",null,"L-0340045 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112120118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-09","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01601669","Sample-Routine","Water","Groundwater","2016-02-10","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374109121000101",null,"L-0430204 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-106942769","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Data reload to update DQI codes per NWQL Rapi-Note 16-28",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-02-19","see result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01601516","Sample-Routine","Water","Groundwater","2016-06-13","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-254934080250401",null,"L-2608734 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-109248816","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-06-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OR","USGS Oregon Water Science Center","nwisor.01.01600402","Sample-Routine","Water","Groundwater","2016-07-13","09:00:00","PDT",{"$nulls":4},300,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-452550117152001",null,"L-1960139 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Other","NWIS-110441435","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2016-07-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01701322","Sample-Routine","Water","Groundwater","2017-01-19","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385801121055801",null,"L-0200032 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-112138350","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-01-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800068","Sample-Routine","Water","Groundwater","2017-10-19","09:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382600121305501",null,"L-2930055 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110972986","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700553","Sample-Routine","Water","Groundwater","2017-08-01","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-392853075005801",null,"L-2349602 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108379633","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703760","Sample-Routine","Water","Groundwater","2017-08-08","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305904103534001",null,"L-2210182 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108588995","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01701317","Sample-Routine","Water","Groundwater","2017-08-10","09:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-414540075453201",null,"L-2230184 WHOI comment: \"Bottle broken but sample intact.\" KB 8/14/17 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108469303","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01702592","Sample-Routine","Water","Groundwater","2017-08-02","09:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-421130076254201",null,"L-2150079 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-108698032","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01702797","Sample-Routine","Water","Groundwater","2017-09-27","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424631073391401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-109098848","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707839","Quality Control Sample-Field Replicate","Water","Groundwater","2017-09-20","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-385200120000001",null,"L-2650153 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115691020","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-23",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01702927","Sample-Routine","Water","Groundwater","2017-02-22","12:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-334700116100001",null,"L-1388703 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-110780380","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-02-27",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707311","Sample-Routine","Water","Groundwater","2017-08-24","13:20:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-382404121250201",null,"L-2370018 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110968136","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.01701323","Sample-Routine","Water","Groundwater","2017-08-14","13:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-415827075560001",null,"L-2270214 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-108511778","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707677","Sample-Routine","Water","Groundwater","2017-09-12","14:00:00","PDT",{"$nulls":4},160,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-384455121292101",null,"L-2560095 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110970496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01702158","Sample-Routine","Water","Groundwater","2017-04-10","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-305624097321101",null,"L-1010241 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-107601248","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-04-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703756","Sample-Routine","Water","Groundwater","2017-06-07","11:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-302646099481501",null,"L-1590298 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-108587112","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01701579","Sample-Routine","Water","Groundwater","2017-03-07","11:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-291943099163301",null,"L-0670023 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-106974659","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-03-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01706099","Sample-Routine","Water","Groundwater","2017-06-28","10:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-342123119024201",null,"L-1810267 X=no date, time, or STA ID on GCC  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115683481","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700639","Sample-Routine","Water","Groundwater","2017-08-21","14:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394604075003601",null,"L-2360059 X=DOC not received.  Deleted LC2612. 8/25/2017 mec  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-108554127","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01707116","Sample-Routine","Water","Groundwater","2017-08-07","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381731121183001",null,"L-2210049 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-110967723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01800670","Sample-Routine","Water","Groundwater","2017-12-18","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-423523076220902",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-109375376","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-12-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TN","USGS Tennessee Water Science Center","nwistn.01.01700138","Sample-Routine","Water","Groundwater","2017-08-16","14:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-351113089513401",null,"L-2300038 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-108568946","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-08-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CT","USGS Connecticut Water Science Center","nwisma.01.01700616","Sample-Routine","Water","Groundwater","2017-04-10","11:00:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-414245072333901",null,"L-1020045 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Jet pump","NWIS-107305888","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-04-13",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700461","Sample-Routine","Water","Groundwater","2017-06-19","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394255075030401",null,"L-2059601 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107897603","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01703761","Sample-Routine","Water","Groundwater","2017-06-28","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303418100382101",null,"L-1800327 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Line-shaft turbine pump","NWIS-108595352","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-UT","USGS Utah Water Science Center","nwisut.01.01701204","Sample-Routine","Water","Groundwater","2017-07-19","11:00:00","MDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381034109274501",null,"L-2010187 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible positive-pressure pump","NWIS-108424763","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-07-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01800041","Sample-Routine","Water","Groundwater","2017-10-12","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-324400114380001",null,"L-2860114 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115691538","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-10-19",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700462","Sample-Routine","Water","Groundwater","2017-06-21","09:40:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394321075015701",null,"L-2059602 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-107897803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-06-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01700658","Sample-Routine","Water","Groundwater","2017-08-24","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-394340075012701",null,"L-2909608 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-108621234","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2017-09-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AZ","USGS Arizona Water Science Center","nwisaz.01.01800155","Sample-Routine","Water","Groundwater","2018-03-28","11:00:00","MST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-332918112283301",null,"L-0880139 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110563647","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-30",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MO","USGS Missouri Water Science Center","nwismo.01.01801082","Sample-Routine","Water","Groundwater","2018-06-19","09:20:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-395012094540101",null,"L-1710072 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8030,"USGS parameter code 82398","Grab sample at water-supply tap",null,"Submersible gear pump","NWIS-111193961","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NJ","USGS New Jersey Water Science Center","nwisnj.01.01800927","Sample-Routine","Water","Groundwater","2018-09-17","13:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-393035074533601",null,"L-2610069 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Submersible centrifugal pump","NWIS-111828227","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-ND","USGS North Dakota Water Science Center","nwisnd.01.01800726","Sample-Routine","Water","Groundwater","2018-07-19","13:00:00","CDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-475427103361401",null,"L-2198712 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111319515","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-07-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01805847","Sample-Routine","Water","Groundwater","2018-09-12","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-363500118140001",null,"L-2570171 Add District Contact RHKENT to ASR.  KMS, 9/17/18  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4100,"USGS parameter code 82398","Flowing well",null,"Flowing well","NWIS-118317003","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.01801656","Sample-Routine","Water","Groundwater","2018-03-13","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-293745098162001",null,"L-0730036 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-110505318","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01900247","Sample-Routine","Water","Groundwater","2018-11-20","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-434803075402901",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-115483496","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802025","Sample-Routine","Water","Groundwater","2018-02-26","09:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345455117052601",null,"L-0600042 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116128032","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01800229","Sample-Routine","Water","Groundwater","2018-06-27","12:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-452350093510301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111216564","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-KS","USGS Kansas Water Science Center","nwisks.01.01801150","Sample-Routine","Water","Groundwater","2018-07-16","10:00:00","CDT",{"$nulls":4},18.2,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Kansas Water Science Center","USGS-372329097105501",null,"L-1980207 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-111289558","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-07-19",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01900338","Sample-Routine","Water","Groundwater","2018-10-23","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-340742116053201",null,"L-2990163 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-118324607","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802022","Sample-Routine","Water","Groundwater","2018-02-27","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-344856116373901",null,"L-0600048 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116127619","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01900033","Sample-Routine","Water","Groundwater","2018-10-03","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-440207075402801",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-112069783","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-10-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802942","Sample-Routine","Water","Groundwater","2018-04-05","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370145121560101",null,"L-1638708 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115702173","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-04-27","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01802023","Quality Control Sample-Field Replicate","Water","Groundwater","2018-02-27","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-344927116394101",null,"L-0600044 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-115697800","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-03-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01801534","Sample-Routine","Water","Groundwater","2018-01-29","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-345245116435801",null,"L-0330077 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116125556","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-02-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01803340","Sample-Routine","Water","Groundwater","2018-04-16","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-343953118041901",null,"L-1100101 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-115954750","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-04-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MN","USGS Minnesota Water Science Center","nwismn.01.01800232","Sample-Routine","Water","Groundwater","2018-06-26","10:30:00","CDT",{"$nulls":4},4.3,"feet",{"$nulls":5},"National Water Quality Assessment Program (NAWQA)",null,"USGS - Minnesota Water Science Center","USGS-452036093423701",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-111217532","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-06-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01805759","Sample-Routine","Water","Groundwater","2018-08-29","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-375100119560001",null,"L-2430110 X=time on samples is 1500, no sta id, date or time on GCC.  Added project chief RHKENT. 9/5/2018 mec  Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-118319878","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-09-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01900104","Sample-Routine","Water","Groundwater","2018-10-30","09:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-412418074244202",null,"L-3068501 Updated SID/SID Name from 412309074264203/O 222 per D. Jensen. JPC 5/21/19  Updated SID from 412309074264203 per K. Colella. JPC 11/8/18",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-112211703","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2018-11-03",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.01902411","Sample-Routine","Water","Groundwater","2019-09-24","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-310934081404801",null,"L-2758702 Samples were received chilled at the WHOI lab. L-2680141 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117842931","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906976","Quality Control Sample-Field Replicate","Water","Groundwater","2019-09-25","13:50:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380337121301001",null,"L-2700098 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124193054","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-10-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906863","Quality Control Sample-Field Replicate","Water","Groundwater","2019-09-10","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374824120503001",null,"L-2540074 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118732780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01902574","Sample-Routine","Water","Groundwater","2019-09-11","10:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USEPA-403132080374501",null,"L-2550043 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117750949","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.01902529","Sample-Routine","Water","Groundwater","2019-09-04","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USEPA-395803081593401",null,"L-2490059 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-117686292","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-11",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902080","Sample-Routine","Water","Groundwater","2019-06-20","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-420134070432301",null,"L-1728502 X = Time on RU looks like 2100.",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-116954541","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-06-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.01901186","Sample-Routine","Water","Groundwater","2019-04-04","15:00:00","EDT",{"$nulls":4},8,"feet",null,7.92,"feet",12.92,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-262854081241301",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-117396044","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-04-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01902596","Sample-Routine","Water","Groundwater","2019-02-28","09:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401754122161601",null,"L-0630002 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118297980","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-03-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01902599","Quality Control Sample-Field Replicate","Water","Groundwater","2019-02-26","12:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401501122285301",null,"L-0590004 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118298825","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-03-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906468","Quality Control Sample-Field Replicate","Water","Groundwater","2019-08-19","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380434120544601",null,"L-2330139 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118734985","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01903540","Sample-Routine","Water","Groundwater","2019-03-26","12:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-403032122193301",null,"L-0880115 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118302810","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-04-05",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NH","USGS New Hampshire Water Science Center","nwisma.01.01902643","Sample-Routine","Water","Groundwater","2019-08-08","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-423713070481301",null,"L-2250079 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Routine sample",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-117610655","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.01901943","Sample-Routine","Water","Groundwater","2019-07-15","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-433320073153401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-117195965","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-07-20",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000381","Sample-Routine","Water","Groundwater","2019-10-30","15:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-263000081390001",null,"L-3040027 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118426130","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IN","USGS Indiana Water Science Center","nwisin.01.01901101","Sample-Routine","Water","Groundwater","2019-09-19","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-385053084485901",null,"L-2630105 Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-118209563","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-09-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906320","Sample-Routine","Water","Groundwater","2019-08-06","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374909121110101",null,"L-2190044 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118737827","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-10",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01903538","Sample-Routine","Water","Groundwater","2019-03-27","13:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-402348122112701",null,"L-0880117 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118302241","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-04-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02000375","Sample-Routine","Water","Groundwater","2019-10-29","17:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-262500081430001",null,"L-3030196 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118424870","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-11-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IN","USGS Indiana Water Science Center","nwisin.01.01901088","Sample-Routine","Water","Groundwater","2019-08-21","12:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-375327087030301",null,"MM-57883A",null,"Not applicable","Not applicable",null,null,8040,"USGS parameter code 82398","Spigot",null,"Mulitple samplers used","NWIS-117753455","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01906315","Sample-Routine","Water","Groundwater","2019-08-08","14:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380919121043901",null,"L-2210101 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118739411","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-08-15",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.01901608","Sample-Routine","Water","Groundwater","2019-02-05","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-365700120220001",null,"L-0390030 Received 3/19/2019 chilled. Samples were received chilled at the WHOI lab.",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-118034474","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2019-02-14",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-OH","USGS Ohio Water Science Center","nwisoh.01.02100016","Sample-Routine","Water","Groundwater","2020-10-14","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-400642083441601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible gear pump","NWIS-119904717","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-10-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100722","Sample-Routine","Water","Groundwater","2020-12-03","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-374240120432601",null,"L-3390097 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122456079","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-12-08",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001510","Quality Control Sample-Field Replicate","Water","Groundwater","2020-01-15","09:50:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-335727116524701",null,"L-0170105 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120719027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"The holding time for the processing of this sample has been exceeded",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-02-01","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001725","Sample-Routine","Water","Groundwater","2020-07-23","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-444454075075401",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119361877","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02001992","Sample-Routine","Water","Groundwater","2020-02-24","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-334031116151201",null,"L-0590103 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120713674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-03-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003425","Sample-Routine","Water","Groundwater","2020-07-22","09:00:00","PDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-334350117553201",null,"L-2100022 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-119368581","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":9},"Hold time parameters were exceeded during the collection to analysis phase of sample processing.",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02100516","Sample-Routine","Water","Groundwater","2020-11-16","14:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-405600123370001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122575031","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-11-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-FL","USGS Florida Water Science Center","nwisfl.01.02100358","Sample-Routine","Water","Groundwater","2020-10-29","10:00:00","EDT",{"$nulls":4},13.5,"feet",{"$nulls":7},"U.S. Geological Survey-Water Resources Discipline","USGS-261525080165101",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120385035","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-10-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001860","Sample-Routine","Water","Groundwater","2020-08-03","10:30:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-420125074474901",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119547118","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001781","Sample-Routine","Water","Groundwater","2020-08-17","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-415601074544901",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119479317","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003635","Sample-Routine","Water","Groundwater","2020-07-21","10:15:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-380948121360901",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-120694374","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02001736","Sample-Routine","Water","Groundwater","2020-07-27","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425825077422201",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-119400094","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003639","Sample-Routine","Water","Groundwater","2020-07-15","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-341400116510001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-120695609","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-07-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100024","Sample-Routine","Water","Groundwater","2020-10-26","13:00:00","CDT",{"$nulls":6},"Below land-surface datum",100,"feet",95,"feet",null,null,"U.S. Geological Survey","USGS-301618092035701",null,"L-3010127 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Jet pump","NWIS-119955663","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-10-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02000346","Sample-Routine","Water","Groundwater","2020-07-29","11:00:00","CDT",{"$nulls":6},"Below land-surface datum",140,"feet",150,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-305020093003001",null,"L-2120201 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4090,"USGS parameter code 82398","Jet pump",null,"Jet pump","NWIS-119388926","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02003821","Sample-Routine","Water","Groundwater","2020-08-17","10:00:00","PDT",{"$nulls":13},"USGS - California Water Science Center","USGS-360000120540001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-121372371","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2020-08-26",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02104660","Sample-Routine","Water","Groundwater","2021-07-14","09:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-390900122030001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-125820083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-07-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02103882","Sample-Routine","Water","Groundwater","2021-06-08","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-335710118211801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-125826372","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102573","Sample-Routine","Water","Groundwater","2021-03-31","14:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-352900119320001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Line-shaft turbine pump","NWIS-122875357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-04-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100260","Sample-Routine","Water","Groundwater","2021-06-15","14:00:00","CDT",{"$nulls":4},45,"feet",null,46,"feet",56,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-301234092012401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121294431","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-23","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101968","Sample-Routine","Water","Groundwater","2021-02-24","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-372746120443601",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-122467130","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-03-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02102114","Sample-Routine","Water","Groundwater","2021-03-08","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-373647120273801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122468715","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-03-18",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101909","Sample-Routine","Water","Groundwater","2021-02-16","11:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-360945119200001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-122824775","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100263","Sample-Routine","Water","Groundwater","2021-06-16","15:00:00","CDT",{"$nulls":4},45,"feet",null,47,"feet",67,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-300932092003801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121295109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-06-25","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101866","Sample-Routine","Water","Groundwater","2021-07-29","09:15:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-423200078250001",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-121686858","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-08-04","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101333","Sample-Routine","Water","Groundwater","2021-01-12","13:40:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-392600121100001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122737291","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-01-22",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.02100348","Sample-Routine","Water","Groundwater","2021-05-20","09:00:00","CST",{"$nulls":4},20,"feet",null,23.08,"feet",28.08,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-425913088133801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122722743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-05-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101595","Quality Control Sample-Field Replicate","Water","Groundwater","2021-01-27","14:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371832120231201",null,"L-0320024 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-122463327","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-04",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101658","Sample-Routine","Water","Groundwater","2021-02-09","13:30:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-371555120285101",null,"L-0530056 Numerical result and or metadata revised; see NWQL Technical Memorandum 2022.01",null,"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-122464276","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":9},"Hold time parameters were exceeded during the collection to analysis phase of sample processing.",68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-24","holding time exceededsee result laboratory comment",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02101907","Sample-Routine","Water","Groundwater","2021-02-17","10:00:00","PST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-362128119390001",{"$nulls":3},"Not applicable","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Line-shaft turbine pump","NWIS-122824150","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-02-25",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02101966","Sample-Routine","Water","Groundwater","2021-09-13","11:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424235078323101",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-121900574","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-LA","USGS Louisiana Water Science Center","nwisla.01.02100226","Sample-Routine","Water","Groundwater","2021-05-26","15:00:00","CDT",{"$nulls":4},38,"feet",null,41,"feet",51,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-300824091593201",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-121167201","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2021-05-28",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02202669","Sample-Routine","Water","Groundwater","2022-03-15","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-353024119213401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125814561","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-03-29",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-MD","USGS Maryland Water Science Center","nwismd.01.02200593","Sample-Routine","Water","Groundwater","2022-08-31","10:30:00","EST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey","USGS-384645076044401",{"$nulls":3},"Not determined","Not applicable",null,null,4045,"USGS parameter code 82398","Submersible multiple impeller (turbine) pump",null,"Suction pump","NWIS-124281604","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-07",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02205688","Sample-Routine","Water","Groundwater","2022-08-29","12:30:00","PDT",{"$nulls":14},"USGS-370625121370401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125806006","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-06",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-TX","USGS Texas Water Science Center","nwistx.01.02300377","Sample-Routine","Water","Groundwater","2022-10-18","09:00:00","CDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-303809097404701",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124641880","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-10-27","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201195","Sample-Routine","Water","Groundwater","2022-07-28","10:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-424544076371801",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-124060406","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-02","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-GA","USGS Georgia Water Science Center","nwisga.01.02201622","Sample-Routine","Water","Groundwater","2022-06-28","16:00:00","EDT",{"$nulls":6},"Below land-surface datum",162.17,"feet",232.92,"feet",null,null,"U.S. Geological Survey-Water Resources Discipline","USGS-332137081581301",null,null,"Midville Aquifer System","Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-124096086","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-07-01",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-AL","USGS Alabama Water Science Center","nwisal.01.02200022","Sample-Routine","Water","Groundwater","2022-03-07","13:00:00","CST",{"$nulls":4},17,"feet",null,14,"feet",24,"feet","National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-344124086531401",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-123779311","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-03-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-VA","USGS Virginia Water Science Center","nwisva.01.02200511","Sample-Routine","Water","Groundwater","2022-04-04","11:00:00","EDT",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-365751076363001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-123455480","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-04-09",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203906","Sample-Routine","Water","Groundwater","2022-05-17","10:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-384814123044001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125236430","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-05-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02204512","Sample-Routine","Water","Groundwater","2022-06-07","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381344122202901",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125239703","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-21",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201194","Sample-Routine","Water","Groundwater","2022-07-27","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-425855075512201",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"None","NWIS-124060123","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-02","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02205771","Sample-Routine","Water","Groundwater","2022-09-13","09:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-370126121301001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125803661","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-09-17",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02300256","Sample-Routine","Water","Groundwater","2022-10-25","11:00:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-333130114394001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible centrifugal pump","NWIS-125801157","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-11-02","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201423","Sample-Routine","Water","Groundwater","2022-08-09","09:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-434343074033101",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124116756","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-16",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-NY","USGS New York Water Science Center","nwisny.01.02201653","Quality Control Sample-Field Replicate","Water","Groundwater","2022-08-24","08:00:00","EST",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-431001076243501",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-124616989","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-08-31",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-CA","USGS California Water Science Center","nwisca.01.02203914","Sample-Routine","Water","Groundwater","2022-05-25","11:30:00","PDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-381448122542001",{"$nulls":3},"Not applicable","Not applicable",null,null,4040,"USGS parameter code 82398","Submersible pump",null,"Submersible positive-pressure pump","NWIS-125236208","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Accepted",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2022-06-02",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.02301802","Sample-Routine","Water","Groundwater","2023-08-02","12:30:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-402119075112801",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-126006339","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-12","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-IL","USGS Illinois Water Science Center","nwisil.01.02300581","Sample-Routine","Water","Groundwater","2023-08-22","10:00:00","CST",{"$nulls":11},"National Water Quality Assessment Program (NAWQA)",null,"U.S. Geological Survey-Water Resources Discipline","USGS-395521088344201",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-126221076","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-24",null,null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["USGS-PA","USGS Pennsylvania Water Science Center","nwispa.01.02301769","Sample-Routine","Water","Groundwater","2023-07-26","10:00:00","EDT",{"$nulls":13},"U.S. Geological Survey-Water Resources Discipline","USGS-401405075275101",{"$nulls":3},"Not applicable","Not applicable",null,null,"USGS","USGS","USGS",null,"Unknown","NWIS-125970134","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Preliminary",null,"Actual",{"$nulls":10},68726,{"$nulls":8},"GCM66","USGS","VOC, wu, acidified, GCMS",null,"USGS OF 97-829","USGS-National Water Quality Lab, Denver, CO","2023-08-04","lab control sample (LCS) recovery outside of range or criteria",null,"Reporting limit by DQCALC",0.08,"ug/l",{"$nulls":4},"NWIS"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW04-VP-D010-062004-0","Sample","Air","Ambient Air","2004-06-30","09:20:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW04",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047849452.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-07-12",{"$nulls":3},2.1,"ppb",1.05,"ppb",null,null,"STORET"]
["INTRMTN","Superfund Intermountain Waste Oil Refinery","INTRMTN-MW07-VP-S001-052004-0","Sample","Air","Ambient Air","2004-05-18","15:02:00","MST",{"$nulls":11},"IWOR8",null,null,"INTRMTN-IWORMW07",{"$nulls":7},"UNKNOWN","UNKNOWN","UNKNOWN",null,"Unknown","STORET-100047852244.0000000000","*Non-detect",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"TO-15","INTRMTN",{"$nulls":4},"2004-05-23",{"$nulls":3},38,"ppb",19,"ppb",null,null,"STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-95543R-gwdb","Sample-Routine","Water","Groundwater","2011-10-28","09:30:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-77503","CLEAN HARBORS AZ CH-4",{"$nulls":4},33.4421758,-112.0904453,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-492536578","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2011-11-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-95543R-gwdb/results/492536578/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2015-12-04T11:52:06","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120443R-gwdb","Sample-Other","Water","Groundwater","2013-08-01","15:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79321","ADEQ IW-1S",{"$nulls":4},33.5244364,-112.0817139,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490947484",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-04",{"$nulls":8},"2015-11-30T18:43:10","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120268R-gwdb","Sample-Other","Water","Groundwater","2013-08-01","12:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490859446",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-08-04",{"$nulls":8},"2015-11-30T17:54:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120359R-gwdb","Sample-Other","Water","Groundwater","2013-12-16","07:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490802011","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-12-22",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120359R-gwdb/results/490802011/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T17:14:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120279.CHEM","Sample-Routine","Other",null,"2013-08-01","11:20:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-53578",64410,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725051519","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120279.CHEM/results/725051519/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2018-05-10T17:39:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120314.CHEM","Sample-Routine","Other",null,"2013-08-01","02:05:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-52553",62913,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.52445,-112.0817647,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725053568","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120314.CHEM/results/725053568/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2018-05-10T17:39:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-120442.CHEM","Sample-Routine","Other",null,"2013-08-01","02:35:00","EST",{"$nulls":4},95,"ft",{"$nulls":5},9426,"2013-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-58790",79323,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5244922,-112.0817217,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725056945","Present Below Quantification Limit",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2013-08-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-120442.CHEM/results/725056945/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2018-05-10T17:40:25","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132031-gwdb","Sample-Routine","Water","Groundwater","2013-09-11","12:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79229","ADEQ MW-109",{"$nulls":4},32.2460544,-109.8368444,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490893729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-15",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132031-gwdb/results/490893729/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:19:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132025-gwdb","Sample-Routine","Water","Groundwater","2013-09-10","13:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79231","ADEQ MW-111",{"$nulls":4},32.2457594,-109.8359936,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490962368","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-09-14",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132025-gwdb/results/490962368/resdetectqntlmts","Lower Reporting Limit",0.02,"mg/L",{"$nulls":3},"2015-11-30T18:49:39","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120478R-gwdb","Sample-Other","Water","Groundwater","2013-10-30","11:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-79322","ADEQ IW-1D",{"$nulls":4},33.5244397,-112.0816878,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490769095",null,null,"1,3-Butadiene","Total",2E-3,"mg/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2013-11-03",{"$nulls":8},"2015-11-30T16:47:56","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-120333R-gwdb","Sample-Other","Water","Groundwater","2014-01-27","09:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64410","ADEQ MW-5",{"$nulls":4},33.5247,-112.0819611,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490942682","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-01-31",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-120333R-gwdb/results/490942682/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:41:31","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122435-gwdb","Sample-Routine","Water","Groundwater","2014-09-24","11:44:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79236","ADEQ MW-116",{"$nulls":4},32.2454761,-109.8358558,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490880201","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-10-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122435-gwdb/results/490880201/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:10:08","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122139-gwdb","Sample-Routine","Water","Groundwater","2014-03-10","13:58:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64047","COP MW-48",{"$nulls":4},33.5008917,-112.1459333,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490875006",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-14",{"$nulls":8},"2015-11-30T18:05:31","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122147-gwdb","Sample-Routine","Water","Groundwater","2014-03-11","10:25:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-59282","WCP-72M",{"$nulls":4},33.4994497,-112.1465058,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490871679",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-14",{"$nulls":8},"2015-11-30T18:02:07","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-121776-gwdb","Sample-Routine","Water","Groundwater","2014-08-06","07:37:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-64409","ADEQ MW-4",{"$nulls":4},33.5248,-112.0815694,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490946274","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-08-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-121776-gwdb/results/490946274/resdetectqntlmts","Lower Reporting Limit",0.04,"mg/L",{"$nulls":3},"2015-11-30T18:42:38","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132368-gwdb","Sample-Routine","Water","Groundwater","2014-03-04","12:10:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-57556","YELLOW CAB RW-1",{"$nulls":4},32.2267939,-110.9675289,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490882980","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132368-gwdb/results/490882980/resdetectqntlmts","Lower Reporting Limit",0.02,"mg/L",{"$nulls":3},"2015-11-30T18:12:54","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122418-gwdb","Sample-Routine","Water","Groundwater","2014-05-20","12:15:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79264","ADEQ MW-104",{"$nulls":4},32.2674414,-109.8470308,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491017719","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-05-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122418-gwdb/results/491017719/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T19:17:37","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122449-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","11:30:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490877351","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122449-gwdb/results/490877351/resdetectqntlmts","Lower Reporting Limit",0.2,"mg/L",{"$nulls":3},"2015-11-30T18:07:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122128-gwdb","Sample-Routine","Water","Groundwater","2014-03-06","09:40:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-59417","WCP-78",{"$nulls":4},33.5025417,-112.1515417,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-491015285",null,null,"1,3-Butadiene","Total",2,"ug/L",null,"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-12",{"$nulls":8},"2015-11-30T19:16:20","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122443-gwdb","Sample-Routine","Water","Groundwater","2014-03-21","07:58:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79234","ADEQ MW-114",{"$nulls":4},32.2459356,-109.8355467,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490808223","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122443-gwdb/results/490808223/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T17:19:01","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-132478-gwdb","Sample-Routine","Water","Groundwater","2014-12-09","15:05:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490889746","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-12-12",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-132478-gwdb/results/490889746/resdetectqntlmts","Lower Reporting Limit",0.2,"mg/L",{"$nulls":3},"2015-11-30T18:17:17","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-122414-gwdb","Sample-Routine","Water","Groundwater","2014-04-17","14:48:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79262","ADEQ MW-102",{"$nulls":4},32.26686,-109.8468753,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-490957723","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2014-04-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-122414-gwdb/results/490957723/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2015-11-30T18:47:40","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148945-gwdb","Sample-Other","Water","Groundwater","2015-10-22","16:04:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-65186","MW-203M",{"$nulls":4},33.4799944,-112.1385917,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552065549","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148945-gwdb/results/552065549/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T02:28:45","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148929-gwdb","Sample-Other","Water","Groundwater","2015-10-23","14:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-60383","WCP-204",{"$nulls":4},33.4819272,-112.1311575,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551993247","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-27",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148929-gwdb/results/551993247/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T01:47:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150795-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","14:10:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79949","THOMPSON TDI-20",{"$nulls":4},34.9024192,-110.1634028,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552046911","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-11",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150795-gwdb/results/552046911/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2016-05-12T02:20:42","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150784-gwdb","Sample-Routine","Water","Groundwater","2015-12-30","12:00:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-79941","THOMPSON TDI-1",{"$nulls":4},34.9025122,-110.1633353,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552064700","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-01-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150784-gwdb/results/552064700/resdetectqntlmts","Lower Reporting Limit",10,"ug/L",{"$nulls":3},"2016-05-12T02:28:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148329-gwdb","Sample-Routine","Water","Groundwater","2015-09-23","12:59:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79226","ADEQ MW-106",{"$nulls":4},32.2460858,-109.8359989,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552135625","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-03",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148329-gwdb/results/552135625/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T02:58:28","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146182-gwdb","Sample-Routine","Water","Groundwater","2015-03-16","13:45:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-58229","IRA-9",{"$nulls":4},32.27998,-111.0031697,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552150379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-20",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146182-gwdb/results/552150379/resdetectqntlmts","Method Detection Level",2,"ug/L",{"$nulls":3},"2016-05-12T03:08:36","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-144200-gwdb","Sample-Routine","Water","Groundwater","2015-03-25","12:00:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79221","ADEQ MW-101",{"$nulls":4},32.2460864,-109.8363083,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552007178","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-04-04",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-144200-gwdb/results/552007178/resdetectqntlmts","Lower Reporting Limit",0.05,"mg/L",{"$nulls":3},"2016-05-12T01:56:07","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148826-gwdb","Sample-Routine","Water","Groundwater","2015-09-22","09:10:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-80426","KENGLA WELL 3",{"$nulls":4},34.1506231,-109.9747219,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552170565","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-09-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148826-gwdb/results/552170565/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2016-05-12T03:14:19","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148939-gwdb","Sample-Other","Water","Groundwater","2015-10-22","11:47:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57159","WOC MW-06M",{"$nulls":4},33.4839803,-112.1425672,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552171293","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-10-29",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148939-gwdb/results/552171293/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T03:14:34","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-148979-gwdb","Sample-Routine","Water","Groundwater","2015-11-20","08:55:00","MST",{"$nulls":11},"GW","GW",null,"21ARIZ_WQX-79225","ADEQ MW-105",{"$nulls":4},32.2462542,-109.8363478,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552175226","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2015-12-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-148979-gwdb/results/552175226/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T03:15:43","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146160-gwdb","Sample-Routine","Water","Groundwater","2015-03-10","13:55:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-57685","IRA-4",{"$nulls":4},32.2709558,-111.0032325,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551973134","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146160-gwdb/results/551973134/resdetectqntlmts","Method Detection Level",2,"ug/L",{"$nulls":3},"2016-05-12T01:29:46","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-146154-gwdb","Sample-Routine","Water","Groundwater","2015-03-16","10:15:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-36092","VILLA CAPRI  WELL",{"$nulls":4},32.2928333,-111.0141389,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552157751","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Qualifier:   ANALYTE REPORTED TO MDL PER PROJECT SPECIFICATION.  TARGET ANALYTE WAS NOT DETECTED IN THE SAMPLE.",{"$nulls":9},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Test America Laboratory - Phoenix","2015-03-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-146154-gwdb/results/552157751/resdetectqntlmts","Method Detection Level",2,"ug/L",{"$nulls":3},"2016-05-12T03:11:00","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-147255-gwdb","Sample-Other","Water","Groundwater","2015-03-20","14:12:00","MST",{"$nulls":11},"MISC","MISC",null,"21ARIZ_WQX-59292","HSMW-5U",{"$nulls":4},33.39371,-111.9388003,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-551984363","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Xenco Laboratories","2015-03-25",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-147255-gwdb/results/551984363/resdetectqntlmts","Lower Reporting Limit",5,"ug/L",{"$nulls":3},"2016-05-12T01:39:09","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-150946-gwdb","Sample-Routine","Water","Groundwater","2016-03-02","13:25:00","MST",{"$nulls":11},"LUST","LUST",null,"21ARIZ_WQX-80597","MW-6A",{"$nulls":4},33.4928372,-113.1617644,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552020148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-150946-gwdb/results/552020148/resdetectqntlmts","Lower Reporting Limit",2,"ug/L",{"$nulls":3},"2016-05-12T02:03:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155338.CHEM","Sample-Routine","Other",null,"2016-08-09","08:25:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58754",79229,{"$nulls":4},32.2460544,-109.8368444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676181821","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-08-17",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155338.CHEM/results/676181821/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2017-11-03T10:08:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-150947.CHEM","Sample-Routine","Other",null,"2016-03-03","08:50:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59190",80594,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.492975,-113.1617631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707988435","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-03-07",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-150947.CHEM/results/707988435/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-03-13T10:39:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155331.CHEM","Sample-Routine","Other",null,"2016-09-14","10:48:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58747",79222,{"$nulls":4},32.2461081,-109.8364322,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676199676","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-09-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155331.CHEM/results/676199676/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2017-11-03T10:11:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155729.CHEM","Sample-Routine","Other",null,"2016-05-03","10:24:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59320",81183,{"$nulls":4},34.5619778,-112.4865694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676260446","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-05-09",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155729.CHEM/results/676260446/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",{"$nulls":3},"2017-11-03T10:24:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156913.CHEM","Sample-Routine","Other",null,"2016-12-06","08:58:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59190",80594,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.492975,-113.1617631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993271","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156913.CHEM/results/707993271/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-03-13T10:41:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156922.CHEM","Sample-Routine","Other",null,"2016-12-05","01:43:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59189",80593,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4927864,-113.1616206,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993964","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156922.CHEM/results/707993964/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-03-13T10:41:18","STORET"]
["21ARIZ_WQX","Arizona Department Of Environmental Quality","21ARIZ_WQX-151704-gwdb","Sample-Other","Water","Groundwater","2016-03-16","14:58:00","MST",{"$nulls":11},"WQRF","WQRF",null,"21ARIZ_WQX-58082","WOC MW-201S",{"$nulls":4},33.4803331,-112.136605,"AZDEQ SOPs","21ARIZ_WQX","AZDEQ Standard Operating Procedures",null,"Water Bottle","STORET-552124379","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Actual",{"$nulls":19},"EPA 8260B","21ARIZ_WQX","VOLATILE ORGANIC COMPOUNDS BY GC/MS",null,null,"Environmental Science Corporation","2016-03-28",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/21ARIZ_WQX/activities/21ARIZ_WQX-151704-gwdb/results/552124379/resdetectqntlmts","Lower Reporting Limit",2E-3,"mg/L",{"$nulls":3},"2016-05-12T02:53:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156041.CHEM","Sample-Routine","Other",null,"2016-09-21","02:01:00","EST",{"$nulls":4},105,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","URS CONSULTANTS","AZDEQ_WPD-58793",79326,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.524588,-112.0825932,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725065646","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX","2016-09-23",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156041.CHEM/results/725065646/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-05-10T17:42:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-151702.CHEM","Sample-Routine","Water","Groundwater","2016-03-16","11:53:00","EST",{"$nulls":4},155,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","ARCADIS G&M, INC.","AZDEQ_WPD-55160",67698,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.4773702,-112.1464663,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-799539083","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-03-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-151702.CHEM/results/799539083/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2019-10-07T11:07:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-155321.CHEM","Sample-Routine","Other",null,"2016-09-13","12:00:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-58759",79234,{"$nulls":4},32.2459356,-109.8355467,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676198923","Not Detected",null,"1,3-Butadiene","Total",null,"mg/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-09-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-155321.CHEM/results/676198923/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2017-11-03T10:11:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156252.CHEM","Sample-Routine","Other",null,"2016-10-21","12:20:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9618,"2016-WQARF SAMPLES","URS CONSULTANTS","AZDEQ_WPD-56983",72800,{"$f":"--- SAMPLE TAKEN: Migrated","v":{"$error":"#NAME?"}},{"$nulls":3},33.5244731,-112.0829683,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725065561","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX","2016-10-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156252.CHEM/results/725065561/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-05-10T17:42:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-156916.CHEM","Sample-Routine","Other",null,"2016-12-06","11:46:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59187",80591,"--- SAMPLE TAKEN: Migrated | REPORTING AGENCY: ATC GROUP SERVICES LLC",{"$nulls":3},33.4929192,-113.1616131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-707993502","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2016-12-08",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-156916.CHEM/results/707993502/resdetectqntlmts","Laboratory Reporting Level",200,"ug/L",{"$nulls":3},"2018-03-13T10:41:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-157559.CHEM","Sample-Routine","Other",null,"2017-02-20","03:12:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59320",81183,{"$nulls":4},34.5619778,-112.4865694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676159780","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2017-02-24",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-157559.CHEM/results/676159780/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2017-11-03T09:23:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18224.CHEM","Sample-Routine","Water",null,"2017-12-07","11:45:00","EST",{"$nulls":11},9725,"2017-WQARF SAMPLES","Pinyon Environmental, Inc","AZDEQ_WPD-59111",80227,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1493833,-109.9723306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-786710880","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18224.CHEM/results/786710880/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-05-01T10:07:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-GW-157047.CHEM","Sample-Routine","Other",null,"2017-01-30","02:23:00","EST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS",null,"AZDEQ_WPD-59169",80492,{"$nulls":4},35.1904639,-109.4332189,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-676161070","Not Detected",null,"1,3-Butadiene","Total",null,"ug/L",null,"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION","2017-02-02",null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-GW-157047.CHEM/results/676161070/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2017-11-03T09:23:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18217.CHEM","Sample-Routine","Water",null,"2017-12-03","04:35:00","EST",{"$nulls":11},9725,"2017-WQARF SAMPLES","Pinyon Environmental, Inc","AZDEQ_WPD-59154",80432,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1508222,-109.977025,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-786710362","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18217.CHEM/results/786710362/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-05-01T10:07:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB11228.CHEM","Sample-Routine","Other",null,"2017-10-31","10:55:00","EST",{"$nulls":4},47,"ft",{"$nulls":5},9691,"VRP_0000","CH2M","AZDEQ_WPD-61636",81379,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.939721,-110.302651,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725240834","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"L | QA FLAGS: E8.",null,47,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"XENCO LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB11228.CHEM/results/725240834/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",{"$nulls":3},"2018-05-15T09:02:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB05690.CHEM","Sample-Routine","Other",null,"2017-11-15","11:37:00","EST",{"$nulls":4},145,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-725093105","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,145,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB05690.CHEM/results/725093105/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-05-11T10:34:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30380.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2018-11-16","01:25:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874903957","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30380.CHEM/results/874903957/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2021-02-05T12:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18668.CHEM","Sample-Routine","Water","Groundwater","2018-11-13","04:05:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789184359","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18668.CHEM/results/789184359/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-06-12T10:04:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18669.CHEM","Sample-Routine","Water","Groundwater","2018-11-13","11:30:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183693","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18669.CHEM/results/789183693/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-06-12T10:04:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18667.CHEM","Sample-Routine","Water","Groundwater","2018-11-14","04:05:00","EST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61658",81400,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.15071,-109.9747382,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-789183915","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18667.CHEM/results/789183915/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2019-06-12T10:04:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14390.CHEM","Sample-Routine","Other",null,"2018-02-11","01:30:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61859",81549,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},34.2166806,-114.2024528,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734875908","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14390.CHEM/results/734875908/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2018-09-24T10:46:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14438.CHEM","Sample-Routine","Other",null,"2018-08-15","12:25:00","EST",{"$nulls":4},130,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734865744","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,130,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14438.CHEM/results/734865744/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2018-09-24T10:45:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14059.CHEM","Sample-Routine","Other",null,"2018-02-08","12:00:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61874",81564,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.6230583,-111.7158139,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734915947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14059.CHEM/results/734915947/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2018-09-24T10:51:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14057.CHEM","Sample-Routine","Other",null,"2018-05-24","10:45:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-61925",81613,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},31.9654694,-110.2871444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734911912","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: E8,N1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14057.CHEM/results/734911912/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2018-09-24T10:51:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB14072.CHEM","Sample-Routine","Other",null,"2018-02-02","03:30:00","EST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HGC","AZDEQ_WPD-52797",63335,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-734875637","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G | QA FLAGS: D2,E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ACCUTEST LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB14072.CHEM/results/734875637/resdetectqntlmts","Laboratory Reporting Level",5,"ug/L",{"$nulls":3},"2018-09-24T10:46:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB17533.CHEM","Sample-Routine","Other",null,"2019-02-14","12:03:00","EST",{"$nulls":4},103.32,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-61593",81363,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},33.4274167,-112.0884444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-781050550","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"G",null,103.32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB17533.CHEM/results/781050550/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2019-03-28T10:25:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29058.CHEM","Sample-Routine","Other","Groundwater","2019-12-10","11:12:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859908756","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29058.CHEM/results/859908756/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28844.CHEM","Sample-Routine","Other","Groundwater","2019-10-01","03:43:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856013999","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28844.CHEM/results/856013999/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2020-09-10T09:53:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB18531.CHEM","Sample-Routine","Water","Groundwater","2019-01-10","09:45:00","EST",{"$nulls":4},320,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,{"$f":"--- SAMPLE TAKEN: Yes","v":{"$error":"#NAME?"}},{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-788208661","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,320,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"TEST AMERICA LABORATORY - PHOENIX",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB18531.CHEM/results/788208661/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2019-05-29T09:08:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29083.CHEM","Sample-Routine","Other","Groundwater","2019-12-12","11:27:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859910381","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29083.CHEM/results/859910381/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29063.CHEM","Sample-Routine","Other","Groundwater","2019-12-11","02:44:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909081","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29063.CHEM/results/859909081/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29988.CHEM","Sample-Routine","Water","Groundwater","2019-04-12","08:43:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62349",81845,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7210566,-112.0000018,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872413552","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29988.CHEM/results/872413552/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2021-01-19T10:34:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30395.CHEM","Sample-Routine","Water","Groundwater","2019-11-18","06:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","ARIZONA DEPT OF ENVIRONMENTAL QUALITY","AZDEQ_WPD-61908",81596,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3108433,-111.0353167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-875255291","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30395.CHEM/results/875255291/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2021-02-08T10:56:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28081.CHEM","Sample-Routine","Water","Groundwater","2019-12-03","10:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59156",80434,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1526417,-109.9773944,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804068","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28081.CHEM/results/849804068/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2020-06-22T11:29:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25015.CHEM","Sample-Routine","Water","Groundwater","2019-11-19","09:11:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52799",63337,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2019433,-110.9690472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-827751386","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25015.CHEM/results/827751386/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-03-13T11:23:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29065.CHEM","Sample-Routine","Other","Groundwater","2019-12-10","02:39:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909211","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29065.CHEM/results/859909211/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29067.CHEM","Sample-Routine","Other","Groundwater","2019-12-10","10:45:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-859909341","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"Airtech Environmental Laboratories, LLC",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29067.CHEM/results/859909341/resdetectqntlmts","Laboratory Reporting Level",0.0221,"mg/m3",{"$nulls":3},"2020-10-14T17:37:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26156.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","12:05:00","MST",{"$nulls":4},119,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-51311",61440,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4320528,-112.0987861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832560449","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},119,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26156.CHEM/results/832560449/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-07T11:05:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28845.CHEM","Sample-Routine","Other","Groundwater","2019-10-02","02:20:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-856014067","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28845.CHEM/results/856014067/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2020-09-10T09:53:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29977.CHEM","Sample-Routine","Water","Groundwater","2019-01-31","09:28:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","HYDRO GEO CHEM","AZDEQ_WPD-62348",81844,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7210559,-112.0000017,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872412738","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29977.CHEM/results/872412738/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2021-01-19T10:33:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26166.CHEM","Sample-Routine","Water","Groundwater","2019-12-10","03:32:00","MST",{"$nulls":4},225,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62400",81882,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4270989,-112.0871484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-832561476","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},225,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26166.CHEM/results/832561476/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-07T11:05:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29764.CHEM","Sample-Routine","Water","Groundwater","2020-11-05","10:15:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52862",63334,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2014664,-110.9687608,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871461944","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29764.CHEM/results/871461944/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2020-12-28T09:36:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32893.CHEM","Sample-Routine","Water","Groundwater","2020-10-14","01:20:00","MST",{"$nulls":4},137,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56712",72041,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3582617,-111.8110453,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905983805","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,137,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32893.CHEM/results/905983805/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29269.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","10:27:00","MST",{"$nulls":4},42,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50199",62104,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4877681,-111.9961122,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860613171","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,42,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29269.CHEM/results/860613171/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30370.CHEM","Sample-Routine","Water","Groundwater","2020-11-12","10:30:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58666",79062,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5088167,-112.0496333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-874765561","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30370.CHEM/results/874765561/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2021-02-04T10:52:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29299.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","12:31:00","MST",{"$nulls":4},156,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62051",81662,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4827923,-111.9998295,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616127","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,156,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29299.CHEM/results/860616127/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26382.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2020-03-13","12:00:00","MST",{"$nulls":4},185,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-58425",78221,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4330189,-112.0983989,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839245555","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},185,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26382.CHEM/results/839245555/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-22T09:29:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26379.CHEM","Sample-Routine","Water","Groundwater","2020-03-11","10:00:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9689,"2017-RESOURCE CONSERVATION AND RECOVERY ACT UNIT","ATC GROUP SERVICES LLC","AZDEQ_WPD-62401",81883,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4289567,-112.0911729,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-839248585","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26379.CHEM/results/839248585/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-04-22T09:30:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28091.CHEM","Sample-Routine","Water","Groundwater","2020-04-06","11:40:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-849804808","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28091.CHEM/results/849804808/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2020-06-22T11:29:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32887.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","07:40:00","MST",{"$nulls":4},333,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905983367","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,333,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32887.CHEM/results/905983367/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB26745.CHEM","Sample-Routine","Water","Groundwater","2020-04-07","07:15:00","MST",{"$nulls":4},129,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58623",78963,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3565861,-111.8082917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-844184027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,129,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB26745.CHEM/results/844184027/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2020-04-27T15:05:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30386.CHEM","Sample-Routine","Water","Groundwater","2020-12-16","05:14:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62548",81983,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2126345,-112.7551879,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-875254505","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30386.CHEM/results/875254505/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-02-08T10:56:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29308.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","11:52:00","MST",{"$nulls":4},87.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58925",79644,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4867869,-111.9982147,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,87.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29308.CHEM/results/860616793/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25042.CHEM","Sample-Routine","Water","Groundwater","2020-01-21","12:38:00","MST",{"$nulls":4},13.83,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","WESTERN TECHNOLOGY INC.","AZDEQ_WPD-61725",81432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0346639,-110.7223667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-829101919","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,13.83,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25042.CHEM/results/829101919/resdetectqntlmts","Laboratory Reporting Level",2E-3,"mg/L",{"$nulls":3},"2020-03-18T11:28:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29936.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","12:35:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62548",81983,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2126345,-112.7551879,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-872129395","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29936.CHEM/results/872129395/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-01-12T11:32:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29305.CHEM","Sample-Routine","Water","Groundwater","2020-09-24","09:54:00","MST",{"$nulls":4},220,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62250",81753,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4900805,-111.994688,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860616571","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,220,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29305.CHEM/results/860616571/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB28326.CHEM","Sample-Routine","Water","Groundwater","2020-03-27","10:40:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-50272",60375,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5087536,-112.0739797,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-850123170","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB28326.CHEM/results/850123170/resdetectqntlmts","Laboratory Reporting Level",3.3E-4,"mg/L",{"$nulls":3},"2020-07-06T11:16:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29282.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","12:24:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62050",81661,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4765057,-112.0172709,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860614503","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29282.CHEM/results/860614503/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32877.CHEM","Sample-Routine","Water","Groundwater","2020-11-24","07:21:00","MST",{"$nulls":4},331,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-47634",57289,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271944,-110.8376042,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905982637","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,331,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32877.CHEM/results/905982637/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32896.CHEM","Sample-Routine","Water","Groundwater","2020-10-14","12:12:00","MST",{"$nulls":4},137,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56713",72042,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3622472,-111.8090983,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905984024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,137,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32896.CHEM/results/905984024/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29777.CHEM","Sample-Routine","Water","Groundwater","2020-10-09","11:30:00","MST",{"$nulls":4},117,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54635",62158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.00218,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-871506748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},117,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29777.CHEM/results/871506748/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2020-12-30T18:52:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29313.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","01:36:00","MST",{"$nulls":4},225,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62052",81663,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4730179,-112.0239066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-860617163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,225,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29313.CHEM/results/860617163/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2020-11-02T09:31:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB25648.CHEM","Sample-Routine","Water","Groundwater","2020-02-12","12:00:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52698",63128,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016983,-110.9688897,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-829618457","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB25648.CHEM/results/829618457/resdetectqntlmts","Laboratory Reporting Level",0.33,"ug/L",{"$nulls":3},"2020-03-25T08:43:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32900.CHEM","Sample-Routine","Water","Groundwater","2020-10-14","08:20:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58522",78621,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4462683,-112.35735,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-905984316","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32900.CHEM/results/905984316/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-03T09:45:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB29332.CHEM","Sample-Routine","Water","Groundwater","2020-09-25","10:16:00","MST",{"$nulls":4},71,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50838",60962,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4793619,-112.01496,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919900748","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,71,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB29332.CHEM/results/919900748/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-12-01T09:39:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43750.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-10","12:00:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992951514","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43750.CHEM/results/992951514/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43723.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","01:54:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61627",81371,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49253,-112.00725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992949516","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43723.CHEM/results/992949516/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35354.CHEM","Sample-Routine","Water","Groundwater","2021-12-22","04:29:00","MST",{"$nulls":4},101,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63017",82381,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8793896,-111.735863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994635345","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,V1.",null,101,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35354.CHEM/results/994635345/resdetectqntlmts","Laboratory Reporting Level",2,"ug/L",{"$nulls":3},"2023-12-04T10:15:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30476.CHEM","Sample-Routine","Water","Groundwater","2021-01-21","12:13:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62645",82052,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0184395,-110.6843498,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-879852522","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30476.CHEM/results/879852522/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2021-03-05T16:20:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43500.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","10:14:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-966047266","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43500.CHEM/results/966047266/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-01-30T10:12:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33341.CHEM","Sample-Routine","Water","Groundwater","2021-09-01","10:06:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62874",82245,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2562309,-114.1468746,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916469217","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33341.CHEM/results/916469217/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:15:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36508.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2021-12-03","03:41:00","MST",{"$nulls":4},215.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62912",82282,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5387948,-112.1870131,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937426609","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},215.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36508.CHEM/results/937426609/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2022-05-03T12:38:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB30469.CHEM","Sample-Routine","Water","Groundwater","2021-01-20","06:50:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62642",82049,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0186834,-110.6842638,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-879851885","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB30469.CHEM/results/879851885/resdetectqntlmts","Laboratory Reporting Level",5.98,"ug/L",{"$nulls":3},"2021-03-05T16:20:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33256.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","01:51:00","MST",{"$nulls":4},208,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62251",81754,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4716569,-112.0263153,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916460363","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,208,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33256.CHEM/results/916460363/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33043.CHEM","Sample-Routine","Water","Groundwater","2021-09-08","10:34:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62847",82218,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0268341,-110.7069226,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916456813","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33043.CHEM/results/916456813/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-10-19T11:11:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35007.CHEM","Sample-Routine","Water","Groundwater","2021-12-21","03:35:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52799",63337,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2019433,-110.9690472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994628978","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35007.CHEM/results/994628978/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44882.CHEM","Sample-Routine","Water","Groundwater","2021-06-03","08:29:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62483",81930,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4953,-112.00041,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974184567","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44882.CHEM/results/974184567/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-05T10:03:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38267.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","12:43:00","MST",{"$nulls":4},39.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63106",82432,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2859565,-110.1178806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943317605","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},39.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38267.CHEM/results/943317605/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",{"$nulls":3},"2022-07-05T13:19:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35576.CHEM","Sample-Routine","Water","Groundwater","2021-09-21","08:50:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47010",56622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048881,-112.1491475,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933547117","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35576.CHEM/results/933547117/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-03-25T10:44:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43691.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","01:35:00","MST",{"$nulls":4},228,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61627",81371,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49253,-112.00725,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992947148","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},228,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43691.CHEM/results/992947148/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37344.CHEM","Sample-Routine","Water","Groundwater","2021-10-28","11:04:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943308120","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":19},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37344.CHEM/results/943308120/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-07-05T13:15:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43758.CHEM","Sample-Routine","Water","Groundwater","2021-12-14","03:08:00","MST",{"$nulls":4},120,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63287",82605,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.492633,-112.0111495,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992952106","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},120,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43758.CHEM/results/992952106/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:50","STORET"]
["AZDEQ_GW","AZDEQ_GW","AZDEQ_GW-AB47877.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","11:15:00","MST",{"$nulls":4},168,"ft",{"$nulls":5},9876,"2023_WQARF","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_GW-53299",64038,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4993,-112.1446278,"Unknown","AZDEQ_GW","Unknown",null,"Miscellaneous (Other)","STORET-988029504","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},168,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_GW","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_GW/activities/AZDEQ_GW-AB47877.CHEM/results/988029504/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-09-06T10:11:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33312.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","05:33:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62743",82131,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0191229,-110.6824885,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916500086","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33312.CHEM/results/916500086/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-10-21T10:57:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44883.CHEM","Sample-Routine","Water","Groundwater","2021-05-26","01:19:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-58929",79648,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49366,-112.00463,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974184646","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44883.CHEM/results/974184646/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-05T10:03:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35739.CHEM","Sample-Routine","Water","Groundwater","2021-12-02","08:39:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63069",82403,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483984,-112.149587,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994515857","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35739.CHEM/results/994515857/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-02T11:38:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38274.CHEM","Sample-Routine","Water","Groundwater","2021-09-22","11:30:00","MST",{"$nulls":4},43,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63083",82409,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860822,-110.1179399,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943318123","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},43,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38274.CHEM/results/943318123/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2022-07-05T13:20:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33995.CHEM","Sample-Routine","Water","Groundwater","2021-09-30","10:31:00","MST",{"$nulls":4},73.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-51181",61309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4801809,-112.0133971,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-919900928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,73.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33995.CHEM/results/919900928/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-12-01T09:40:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32936.CHEM","Sample-Routine","Water","Groundwater","2021-08-09","03:09:00","MST",{"$nulls":4},209,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62820",82198,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7652751,-112.4536329,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-914941618","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,209,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32936.CHEM/results/914941618/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-10-01T11:40:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33342.CHEM","Sample-Routine","Water","Groundwater","2021-09-01","07:36:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62673",82078,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2561063,-114.146959,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916469309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5,V1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33342.CHEM/results/916469309/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:15:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33076.CHEM","Sample-Routine","Water","Groundwater","2021-09-14","08:38:00","MST",{"$nulls":4},235,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50237",60340,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3779486,-111.8246017,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916457033","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,235,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33076.CHEM/results/916457033/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:11:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43499.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","09:33:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-966047191","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43499.CHEM/results/966047191/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-01-30T10:12:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32941.CHEM","Sample-Routine","Water","Groundwater","2021-08-09","03:42:00","MST",{"$nulls":4},210,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62826",82204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651708,-112.4536862,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-914941938","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,210,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32941.CHEM/results/914941938/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-10-01T11:40:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36501.CHEM","Sample-Routine","Water","Groundwater","2021-12-03","12:25:00","MST",{"$nulls":4},215,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62916",82286,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5388076,-112.1871246,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937426091","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},215,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36501.CHEM/results/937426091/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-05-03T12:37:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48312.CHEM","Sample-Routine","Water","Groundwater","2021-11-17","09:00:00","MST",{"$nulls":4},125,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63194",82513,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7362398,-112.0100517,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993004319","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},125,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48312.CHEM/results/993004319/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2023-11-09T09:47:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32920.CHEM","Sample-Routine","Water","Groundwater","2021-07-20","08:09:00","MST",{"$nulls":4},345,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-906967356","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,N1.",null,345,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32920.CHEM/results/906967356/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-09T21:59:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35005.CHEM","Sample-Routine","Water","Groundwater","2021-12-19","03:24:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52862",63334,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2014664,-110.9687608,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994628793","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35005.CHEM/results/994628793/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35590.CHEM","Sample-Routine","Water","Groundwater","2021-09-23","10:40:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63056",82390,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484119,-112.1499339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-933548167","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35590.CHEM/results/933548167/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-03-25T10:45:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34976.CHEM","Sample-Routine","Water","Groundwater","2021-12-02","09:47:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62655",82062,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0183469,-110.6844878,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994507876","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34976.CHEM/results/994507876/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2023-12-02T11:38:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34207.CHEM","Sample-Routine","Water","Groundwater","2021-11-16","12:05:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52695",63125,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2026803,-110.9690714,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-925214930","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34207.CHEM/results/925214930/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2021-12-28T10:27:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34175.CHEM","Sample-Routine","Water","Groundwater","2021-11-30","09:41:00","MST",{"$nulls":11},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62875",82246,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2560792,-114.1470676,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994247452","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34175.CHEM/results/994247452/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-30T10:14:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43433.CHEM","Sample-Routine","Water","Groundwater","2021-11-18","01:15:00","MST",{"$nulls":4},295,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62811",82190,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5032469,-112.1732619,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992939378","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},295,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43433.CHEM/results/992939378/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33021.CHEM","Sample-Routine","Water","Groundwater","2021-08-20","03:29:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52797",63335,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916464169","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33021.CHEM/results/916464169/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",{"$nulls":3},"2021-10-19T11:13:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33202.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","06:54:00","MST",{"$nulls":4},148,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62005",81652,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.365538,-111.8222295,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916461251","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,148,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33202.CHEM/results/916461251/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32913.CHEM","Sample-Routine","Water","Groundwater","2021-07-20","06:52:00","MST",{"$nulls":4},330,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62099",81698,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3595803,-110.8348695,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-906966873","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,N1.",null,330,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32913.CHEM/results/906966873/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-09T21:59:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37395.CHEM","Sample-Routine","Water","Groundwater","2021-10-22","12:30:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62249",81752,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5038102,-112.0479517,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943311080","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37395.CHEM/results/943311080/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-07-05T13:16:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34988.CHEM","Sample-Routine","Water","Groundwater","2021-11-30","12:19:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62742",82130,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0197062,-110.68312,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994250696","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34988.CHEM/results/994250696/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-30T10:14:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37340.CHEM","Sample-Routine","Water","Groundwater","2021-10-27","02:00:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59148",80426,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1510806,-109.9747219,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-943307824","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37340.CHEM/results/943307824/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-07-05T13:15:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33253.CHEM","Sample-Routine","Water","Groundwater","2021-09-10","01:07:00","MST",{"$nulls":4},245,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62052",81663,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4730179,-112.0239066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916460141","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,L5.",null,245,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33253.CHEM/results/916460141/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB34061.CHEM","Sample-Routine","Water","Groundwater","2021-11-09","01:56:00","MST",{"$nulls":4},209,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62826",82204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651708,-112.4536862,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-921314941","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,209,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB34061.CHEM/results/921314941/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2021-12-06T09:11:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB32921.CHEM","Sample-Routine","Water","Groundwater","2021-07-20","07:50:00","MST",{"$nulls":4},345,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62133",81708,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2271694,-110.8374424,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-906967425","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8,N1.",null,345,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB32921.CHEM/results/906967425/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-08-09T21:59:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33216.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","10:20:00","MST",{"$nulls":4},142,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-58622",78962,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3597333,-111.8042472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916462287","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,142,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33216.CHEM/results/916462287/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:13:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44914.CHEM","Sample-Routine","Water","Groundwater","2021-05-25","11:26:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54635",62158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.00218,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974187048","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44914.CHEM/results/974187048/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-05T10:07:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43736.CHEM","Sample-Routine","Water","Groundwater","2021-12-08","03:44:00","MST",{"$nulls":4},118,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-40429",46747,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49439,-112.00447,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992950478","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},118,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43736.CHEM/results/992950478/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB33210.CHEM","Sample-Routine","Water","Groundwater","2021-09-16","09:21:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-56714",72043,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3639236,-111.8073342,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-916461843","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",null,135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB33210.CHEM/results/916461843/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2021-10-19T11:12:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38951.CHEM","Sample-Routine","Water","Groundwater","2022-04-01","09:40:00","MST",{"$nulls":4},97,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62940",82306,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834931,-110.7759672,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-950632947","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},97,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38951.CHEM/results/950632947/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-08-30T11:00:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43071.CHEM","Sample-Routine","Water","Groundwater","2022-12-27","04:28:00","MST",{"$nulls":4},43,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62873",82244,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2529041,-110.0338758,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994681324","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4,Q7.",null,43,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43071.CHEM/results/994681324/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:19:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42926.CHEM","Sample-Routine","Water","Groundwater","2022-06-16","10:56:00","MST",{"$nulls":4},500,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63495",82807,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4843917,-111.7324554,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992928137","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,500,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42926.CHEM/results/992928137/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40275.CHEM","Sample-Routine","Water","Groundwater","2022-09-23","03:54:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62546",81981,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2122863,-112.7554876,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956948745","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40275.CHEM/results/956948745/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-10-28T11:00:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43537.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","01:58:00","MST",{"$nulls":4},125,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63304",82622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4921451,-114.3471484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992941820","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,125,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43537.CHEM/results/992941820/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37117.CHEM","Sample-Routine","Water","Groundwater","2022-05-20","02:20:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52816",63357,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016572,-110.9689964,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994653237","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37117.CHEM/results/994653237/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35752.CHEM","Sample-Routine","Water","Groundwater","2022-02-18","05:15:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52797",63335,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2018161,-110.9689972,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994637427","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35752.CHEM/results/994637427/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",{"$nulls":3},"2023-12-04T10:15:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39336.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","10:14:00","MST",{"$nulls":4},172,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62821",82199,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.765276,-112.4536326,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994662250","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,172,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39336.CHEM/results/994662250/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49851.CHEM","Sample-Routine","Water","Groundwater","2022-02-17","12:10:00","MST",{"$nulls":4},227,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63152",82471,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5192136,-112.0810416,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999764669","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,227,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49851.CHEM/results/999764669/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2024-01-19T08:41:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41694.CHEM","Sample-Routine","Water","Groundwater","2022-11-18","09:45:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62647",82054,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0199058,-110.6829579,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994680010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41694.CHEM/results/994680010/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:19:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41241.CHEM","Sample-Routine","Water","Groundwater","2022-06-03","07:55:00","MST",{"$nulls":4},38,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62992",82358,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3360028,-110.9413239,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994673755","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},38,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41241.CHEM/results/994673755/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:18:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48151.CHEM","Sample-Routine","Water","Groundwater","2022-05-12","09:35:00","MST",{"$nulls":4},65,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63191",82510,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7237579,-112.00439,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361026","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},65,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48151.CHEM/results/997361026/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-12-29T09:53:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35266.CHEM","Sample-Routine","Water","Groundwater","2022-02-08","01:28:00","MST",{"$nulls":4},215.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62826",82204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7651708,-112.4536862,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994632940","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,215.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35266.CHEM/results/994632940/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:14:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35758.CHEM","Sample-Routine","Water","Groundwater","2022-02-14","03:21:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52695",63125,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2026803,-110.9690714,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994637994","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35758.CHEM/results/994637994/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:15:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35267.CHEM","Sample-Routine","Water","Groundwater","2022-02-08","09:45:00","MST",{"$nulls":4},205,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62820",82198,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7652751,-112.4536329,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994633004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,205,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35267.CHEM/results/994633004/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:14:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36944.CHEM","Sample-Routine","Water","Groundwater","2022-05-09","09:57:00","MST",{"$nulls":4},205.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62820",82198,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7652751,-112.4536329,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994648250","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,205.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36944.CHEM/results/994648250/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:16:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39476.CHEM","Sample-Routine","Water","Groundwater","2022-09-06","04:38:00","MST",{"$nulls":4},36.8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62868",82239,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2528438,-110.0338152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994663221","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,36.8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39476.CHEM/results/994663221/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40277.CHEM","Sample-Routine","Water","Groundwater","2022-09-22","03:00:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62547",81982,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.212638,-112.7553669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-956948929","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40277.CHEM/results/956948929/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2022-10-28T11:00:30","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39588.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","11:00:00","MST",{"$nulls":4},42,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63095",82421,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860355,-110.1180487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667773","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},42,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39588.CHEM/results/953667773/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",{"$nulls":3},"2022-10-12T10:05:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36021.CHEM","Sample-Routine","Water","Groundwater","2022-03-11","10:46:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62840",82211,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0267533,-110.7072866,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994642426","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: R7.",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36021.CHEM/results/994642426/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37467.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","06:54:00","MST",{"$nulls":4},180,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62692",82097,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5083552,-112.0731066,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902357","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},180,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37467.CHEM/results/992902357/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39197.CHEM","Sample-Routine","Water","Groundwater","2022-08-19","01:47:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62576",82010,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7238778,-111.9985028,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992909186","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39197.CHEM/results/992909186/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48812.CHEM","Sample-Routine","Water","Groundwater","2022-08-30","01:00:00","MST",{"$nulls":4},159,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62560",81995,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945731,-114.6214489,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993010199","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},159,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48812.CHEM/results/993010199/resdetectqntlmts","Laboratory Reporting Level",1.49,"ug/L",{"$nulls":3},"2023-11-09T09:48:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39490.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","09:02:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-50239",60342,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3780447,-111.8244892,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992912071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39490.CHEM/results/992912071/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:37:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40413.CHEM","Sample-Routine","Water","Groundwater","2022-01-17","11:15:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-62424",81900,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0674205,-112.1518977,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999446746","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40413.CHEM/results/999446746/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-16T10:10:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41526.CHEM","Sample-Routine","Water","Groundwater","2022-11-23","01:34:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52698",63128,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016983,-110.9688897,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994676743","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41526.CHEM/results/994676743/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:19:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37140.CHEM","Sample-Routine","Water","Groundwater","2022-05-24","05:17:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62551",81986,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9010599,-110.1597276,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992894596","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37140.CHEM/results/992894596/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:36:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41737.CHEM","Sample-Routine","Water","Groundwater","2022-03-28","07:30:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-5035",10129,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.488105,-111.7301342,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992926257","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41737.CHEM/results/992926257/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41629.CHEM","Sample-Routine","Water","Groundwater","2022-11-30","02:35:00","MST",{"$nulls":4},70.74,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962654831","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},70.74,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41629.CHEM/results/962654831/resdetectqntlmts","Laboratory Reporting Level",29.9,"ug/L",{"$nulls":3},"2023-01-06T10:30:55","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48470.CHEM","Sample-Routine","Water","Groundwater","2022-09-06","09:45:00","MST",{"$nulls":4},164,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61854",81546,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4995459,-112.1452744,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993002017","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},164,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48470.CHEM/results/993002017/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43532.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-08-10","12:00:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62815",82194,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.488799,-114.3461386,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992941450","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43532.CHEM/results/992941450/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37470.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","05:40:00","MST",{"$nulls":4},100,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49517",59450,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5089358,-112.0742047,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902579","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},100,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37470.CHEM/results/992902579/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41631.CHEM","Sample-Routine","Water","Groundwater","2022-11-30","03:24:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62940",82306,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834931,-110.7759672,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-962655010","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41631.CHEM/results/962655010/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-01-06T10:31:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39299.CHEM","Sample-Routine","Water","Groundwater","2022-08-24","05:39:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62638",82045,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0189569,-110.6844168,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994660760","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39299.CHEM/results/994660760/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43890.CHEM","Sample-Routine","Other","Groundwater","2022-11-28","12:24:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992954351","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43890.CHEM/results/992954351/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:42:10","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47535.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","07:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62563",81998,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4994189,-112.1458556,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992988600","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47535.CHEM/results/992988600/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43875.CHEM","Sample-Routine","Water","Groundwater","2022-11-17","10:21:00","MST",{"$nulls":4},110,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61626",81370,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.49403,-112.00375,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992952846","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},110,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43875.CHEM/results/992952846/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:41:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38524.CHEM","Sample-Routine","Water","Groundwater","2022-05-18","03:23:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49182",59108,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2208333,-114.5638889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994658240","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38524.CHEM/results/994658240/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41256.CHEM","Sample-Routine","Water","Groundwater","2022-06-01","05:55:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994674890","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41256.CHEM/results/994674890/resdetectqntlmts","Laboratory Reporting Level",14.9,"ug/L",{"$nulls":3},"2023-12-04T10:19:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40575.CHEM","Sample-Routine","Water","Groundwater","2022-01-25","11:00:00","MST",{"$nulls":4},88,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63517",82829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2122569,-110.9686374,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999758140","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},88,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40575.CHEM/results/999758140/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-19T08:41:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39697.CHEM","Sample-Routine","Other","Groundwater","2022-04-20","01:26:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-954060224","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39697.CHEM/results/954060224/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2022-10-14T11:13:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39219.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","01:45:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62567",82001,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7373778,-112.0074722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992910814","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39219.CHEM/results/992910814/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35000.CHEM","Sample-Routine","Water","Groundwater","2022-01-12","04:05:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-61874",81564,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.6230583,-111.7158139,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994628343","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: M1,M2,R2.",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35000.CHEM/results/994628343/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49116.CHEM","Sample-Routine","Water","Groundwater","2022-09-20","05:22:00","MST",{"$nulls":4},327.5,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62775",82154,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4867908,-112.100564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993015248","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},327.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49116.CHEM/results/993015248/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35497.CHEM","Sample-Routine","Water","Groundwater","2022-03-01","10:28:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62543",81978,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4934,-111.9863,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992884706","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35497.CHEM/results/992884706/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:35:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36044.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-03","12:00:00","MST",{"$nulls":4},16,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47011",56623,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482379,-112.1500859,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994643479","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},16,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36044.CHEM/results/994643479/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43039.CHEM","Sample-Routine","Water","Groundwater","2022-11-05","01:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-53890",64948,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2288028,-110.97026,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992932718","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43039.CHEM/results/992932718/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39303.CHEM","Sample-Routine","Water","Groundwater","2022-08-27","12:12:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62741",82129,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0193875,-110.6822587,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994661128","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39303.CHEM/results/994661128/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37464.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-04-06","12:00:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-49518",59451,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.508745,-112.0739306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992902135","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37464.CHEM/results/992902135/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43545.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","07:09:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63297",82615,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4859476,-114.3529682,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992942412","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,60,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43545.CHEM/results/992942412/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41505.CHEM","Sample-Routine","Water","Groundwater","2022-11-22","02:25:00","MST",{"$nulls":4},38.76,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63095",82421,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2860355,-110.1180487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969238725","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},38.76,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41505.CHEM/results/969238725/resdetectqntlmts","Laboratory Reporting Level",299,"ug/L",{"$nulls":3},"2023-03-03T09:05:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39233.CHEM","Sample-Routine","Water","Groundwater","2022-08-27","04:40:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52690",63120,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016586,-110.9696389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994658711","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39233.CHEM/results/994658711/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40724.CHEM","Sample-Routine","Water","Groundwater","2022-03-22","02:35:00","MST",{"$nulls":4},345,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59141",80388,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4993939,-111.7181111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992920041","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,345,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40724.CHEM/results/992920041/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:38:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41169.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","04:40:00","MST",{"$nulls":4},8,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63057",82391,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483738,-112.1498945,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994670087","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,8,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41169.CHEM/results/994670087/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39222.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","03:05:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62599",82033,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7368583,-112.0076694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992911036","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39222.CHEM/results/992911036/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43229.CHEM","Sample-Routine","Water","Groundwater","2022-10-14","02:30:00","MST",{"$nulls":4},87,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54036",65204,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5087114,-112.0465083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999650799","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},87,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43229.CHEM/results/999650799/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-18T09:30:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39181.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","09:55:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62585",82019,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7239944,-112.0012278,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908002","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39181.CHEM/results/992908002/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43796.CHEM","Sample-Routine","Water","Groundwater","2022-12-07","09:52:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62977",82343,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.335875,-110.9417802,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994685898","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43796.CHEM/results/994685898/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:20:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39188.CHEM","Sample-Routine","Water","Groundwater","2022-08-19","09:20:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62682",82087,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7311444,-112.0063889,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908520","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39188.CHEM/results/992908520/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47539.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","10:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55525",68579,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5005161,-112.1482836,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992988896","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47539.CHEM/results/992988896/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43346.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-03-04","12:00:00","MST",{"$nulls":4},208,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63272",82590,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5167132,-112.176642,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992938268","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},208,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43346.CHEM/results/992938268/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41187.CHEM","Sample-Routine","Water","Groundwater","2022-09-12","12:13:00","MST",{"$nulls":4},100.49,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63018",82382,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8788259,-111.7362534,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994671435","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,100.49,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41187.CHEM/results/994671435/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40676.CHEM","Sample-Routine","Water","Groundwater","2022-05-11","09:13:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63536",82848,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152112,-110.1515416,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994668952","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40676.CHEM/results/994668952/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:18:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43799.CHEM","Sample-Routine","Water","Groundwater","2022-12-07","11:57:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62983",82349,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357611,-110.9416976,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994686122","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43799.CHEM/results/994686122/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:20:04","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36526.CHEM","Sample-Routine","Water","Groundwater","2022-03-09","12:47:00","MST",{"$nulls":4},101,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63021",82385,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.8801621,-111.7359074,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994645679","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,101,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36526.CHEM/results/994645679/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:16:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47502.CHEM","Sample-Routine","Water","Groundwater","2022-04-17","10:00:00","MST",{"$nulls":4},230,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-48036",57704,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2285256,-111.3335314,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992986163","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},230,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47502.CHEM/results/992986163/resdetectqntlmts","Laboratory Reporting Level",0.000299000006634742,"ug/L",{"$nulls":3},"2023-11-09T09:45:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47768.CHEM","Sample-Routine","Water","Groundwater","2022-04-11","02:00:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62521",81958,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.525761,-112.081087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992990083","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47768.CHEM/results/992990083/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37039.CHEM","Sample-Routine","Water","Groundwater","2022-05-10","04:10:00","MST",{"$nulls":4},23,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47008",56620,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0476764,-112.1489107,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650029","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,23,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37039.CHEM/results/994650029/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40416.CHEM","Sample-Routine","Water","Groundwater","2022-01-18","12:00:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-62429",81905,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0683157,-112.1514167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999647398","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40416.CHEM/results/999647398/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-18T09:29:57","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB40667.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","10:24:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63529",82841,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152602,-110.1537538,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994668278","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB40667.CHEM/results/994668278/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:18:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43508.CHEM","Sample-Routine","Water","Groundwater","2022-08-09","04:56:00","MST",{"$nulls":4},155,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62690",82095,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4907601,-114.3477968,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992939674","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},155,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43508.CHEM/results/992939674/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47542.CHEM","Sample-Routine","Water","Groundwater","2022-05-05","08:20:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-53300",64039,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4976944,-112.1456028,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992989119","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47542.CHEM/results/992989119/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:46:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41168.CHEM","Sample-Routine","Water","Groundwater","2022-09-09","01:17:00","MST",{"$nulls":4},24,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63066",82400,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481667,-112.1489083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994670013","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,24,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41168.CHEM/results/994670013/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:18:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43343.CHEM","Sample-Routine","Water","Groundwater","2022-03-04","11:20:00","MST",{"$nulls":4},200,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63274",82592,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4991517,-112.16619180000001,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992938046","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},200,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43343.CHEM/results/992938046/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38582.CHEM","Sample-Routine","Water","Groundwater","2022-06-07","02:48:00","MST",{"$nulls":4},10.9,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62855",82226,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2545888,-110.0306365,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994656309","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},10.9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38582.CHEM/results/994656309/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48156.CHEM","Sample-Routine","Water","Groundwater","2022-05-11","02:20:00","MST",{"$nulls":4},75,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63195",82514,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.736204,-112.010142,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994876152","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},75,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48156.CHEM/results/994876152/resdetectqntlmts","Laboratory Reporting Level",2.99000000953674,"ug/L",{"$nulls":3},"2023-12-06T15:47:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35680.CHEM","Sample-Routine","Water","Groundwater","2022-02-24","04:51:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62779",82158,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.212335,-112.7553257,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994635986","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35680.CHEM/results/994635986/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:15:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37446.CHEM","Sample-Routine","Water","Groundwater","2022-04-07","01:20:00","MST",{"$nulls":4},80,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-54184",61809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5104497,-112.0743658,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992900803","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},80,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37446.CHEM/results/992900803/resdetectqntlmts","Laboratory Reporting Level",2.99E-4,"mg/L",{"$nulls":3},"2023-11-09T09:37:00","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43083.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","10:45:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62099",81698,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.3595803,-110.8348695,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992933753","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43083.CHEM/results/992933753/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:39:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41689.CHEM","Sample-Routine","Water","Groundwater","2022-11-16","03:45:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62644",82051,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.0185409,-110.6841669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994679547","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,9,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41689.CHEM/results/994679547/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2023-12-04T10:19:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41509.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-11-22","01:15:00","MST",{"$nulls":4},32.09,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63092",82418,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2861373,-110.1179947,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-969239052","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},32.09,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41509.CHEM/results/969239052/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-03-03T09:05:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35217.CHEM","Sample-Routine","Water","Groundwater","2022-01-19","06:13:00","MST",{"$nulls":4},25,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-62377",81859,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2205364,-114.5641411,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994631838","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,25,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35217.CHEM/results/994631838/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB36513.CHEM","Sample-Routine","Water","Groundwater","2022-04-06","10:16:00","MST",{"$nulls":4},25.5,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63001",82366,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.5067521,-109.3643126,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-937787377","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},25.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB36513.CHEM/results/937787377/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-05-05T10:33:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43079.CHEM","Sample-Routine","Water","Groundwater","2022-12-06","11:47:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62131",81706,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2272003,-110.8375236,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992933457","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: L, LOW FLOW &/OR MICRO PURGE | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43079.CHEM/results/992933457/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:39:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43510.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","03:31:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63301",82619,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.492867,-114.3461749,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992939822","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: L1.",null,135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43510.CHEM/results/992939822/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38474.CHEM","Sample-Routine","Water","Groundwater","2022-06-20","10:32:00","MST",{"$nulls":4},177.5,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62825",82203,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7648134,-112.4536487,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994655252","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,177.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ORANGE COAST ANALYTICAL LABORATORIES",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38474.CHEM/results/994655252/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:17:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43180.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2022-11-10","01:32:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63065",82399,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0481968,-112.1490371,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994682759","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43180.CHEM/results/994682759/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:19:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43133.CHEM","Sample-Routine","Water","Groundwater","2022-12-16","11:15:00","MST",{"$nulls":4},29,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","TERRACON CONSULTANTS WESTERN","AZDEQ_WPD-63536",82848,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9152112,-110.1515416,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994687914","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},29,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43133.CHEM/results/994687914/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2023-12-04T10:20:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35856.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","12:38:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62993",82359,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357048,-110.9417694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994641295","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35856.CHEM/results/994641295/resdetectqntlmts","Laboratory Reporting Level",7.48,"ug/L",{"$nulls":3},"2023-12-04T10:16:07","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45185.CHEM","Sample-Routine","Water","Groundwater","2022-10-17","05:10:00","MST",{"$nulls":4},120,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63286",82604,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4925483,-112.0072941,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992969367","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},120,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45185.CHEM/results/992969367/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:43:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39191.CHEM","Sample-Routine","Water","Groundwater","2022-08-17","07:40:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62574",82008,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7279944,-112.0014028,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992908742","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39191.CHEM/results/992908742/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:37:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37111.CHEM","Sample-Routine","Water","Groundwater","2022-05-19","02:32:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-52690",63120,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2016586,-110.9696389,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994652684","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,85,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37111.CHEM/results/994652684/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:17:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39572.CHEM","Sample-Routine","Water","Groundwater","2022-09-13","10:35:00","MST",{"$nulls":4},50,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63127",82447,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.7388939,-112.0078414,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953580071","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},50,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39572.CHEM/results/953580071/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-10-07T10:34:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48453.CHEM","Sample-Routine","Water","Groundwater","2022-02-22","11:05:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62161",81716,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5249138,-112.0816383,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993002977","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48453.CHEM/results/993002977/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:47:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB43542.CHEM","Sample-Routine","Water","Groundwater","2022-08-10","02:15:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-63304",82622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.4921451,-114.3471484,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992942190","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB43542.CHEM/results/992942190/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:40:40","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47976.CHEM","Sample-Routine","Water","Groundwater","2022-10-03","11:50:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-56983",72800,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5244731,-112.0829683,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992991387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47976.CHEM/results/992991387/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49843.CHEM","Sample-Routine","Water","Groundwater","2022-02-18","12:45:00","MST",{"$nulls":4},135,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62518",81955,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5257506,-112.0816368,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993026857","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},135,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49843.CHEM/results/993026857/resdetectqntlmts","Laboratory Reporting Level",1,"ug/L",{"$nulls":3},"2023-11-09T09:49:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48457.CHEM","Quality Control Sample-Equipment Blank","Water","Groundwater","2022-02-22","09:15:00","MST",{"$nulls":4},0,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-53578",64410,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993003569","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},0,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48457.CHEM/results/993003569/resdetectqntlmts","Laboratory Reporting Level",0.29899999499321,"ug/L",{"$nulls":3},"2023-11-09T09:47:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB42954.CHEM","Sample-Routine","Water","Groundwater","2022-09-03","09:30:00","MST",{"$nulls":4},73,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59142",80389,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4988708,-111.7143906,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992930705","Not Detected",null,"1,3-Butadiene","Total",null,null,"J","Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES | QA FLAGS: J3.",null,73,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB42954.CHEM/results/992930705/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2023-11-09T09:39:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB35219.CHEM","Sample-Routine","Water","Groundwater","2022-01-21","04:10:00","MST",{"$nulls":4},28,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","HYDRO GEO CHEM","AZDEQ_WPD-49223",59153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},35.2213989,-114.5633969,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994632028","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB",null,28,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB35219.CHEM/results/994632028/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:14:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB38744.CHEM","Sample-Routine","Water","Groundwater","2022-07-20","10:35:00","MST",{"$nulls":11},9749,"2018-WQARF Samples","Wood Environment & Infratructure Solutions","AZDEQ_WPD-62100",81699,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2262032,-110.8349466,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992906299","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: G, GRAB | QA FLAGS: E8.",{"$nulls":9},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Eurofins TestAmerica - Phoenix",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB38744.CHEM/results/992906299/resdetectqntlmts","Laboratory Reporting Level",4,"ug/L",{"$nulls":3},"2023-11-09T09:37:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB39582.CHEM","Sample-Routine","Water","Groundwater","2022-03-16","08:40:00","MST",{"$nulls":4},26,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63089",82415,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2861544,-110.1178365,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-953667329","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},26,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB39582.CHEM/results/953667329/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2022-10-12T10:05:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47985.CHEM","Sample-Routine","Water","Groundwater","2022-10-04","11:00:00","MST",{"$nulls":4},90,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-53578",64410,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5247066,-112.0819891,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992992059","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},90,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47985.CHEM/results/992992059/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47554.CHEM","Sample-Routine","Water","Groundwater","2022-04-29","06:50:00","MST",{"$nulls":4},167,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-59250",81051,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4989258,-112.1439489,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992987785","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},167,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47554.CHEM/results/992987785/resdetectqntlmts","Laboratory Reporting Level",1.49000000953674,"ug/L",{"$nulls":3},"2023-11-09T09:45:58","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB41715.CHEM","Sample-Routine","Water","Groundwater","2022-03-23","02:39:00","MST",{"$nulls":4},312,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-47795",57463,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4750856,-111.7297614,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992924524","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"Sample Purpose: K, DISCRETE INTERVAL SAMPLES",null,312,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB41715.CHEM/results/992924524/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:39:11","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB37040.CHEM","Sample-Routine","Water","Groundwater","2022-05-12","10:49:00","MST",{"$nulls":4},22,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63058",82392,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0482178,-112.1488252,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994650104","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"TOTAL | QA FLAGS: R7.",null,22,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"ENVIRONMENTAL SCIENCE CORPORATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB37040.CHEM/results/994650104/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-12-04T10:16:56","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45342.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","08:25:00","MST",{"$nulls":4},50.6,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-63097",82423,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2863196,-110.1181009,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974804387","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},50.6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45342.CHEM/results/974804387/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-05-23T13:51:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47276.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","12:35:00","MST",{"$nulls":4},175,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62266",81767,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6944968,-114.6203508,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999215537","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},175,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47276.CHEM/results/999215537/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-09T09:21:02","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47281.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","11:30:00","MST",{"$nulls":4},153,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62557",81992,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6951457,-114.6203806,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999215909","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},153,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47281.CHEM/results/999215909/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-09T09:21:05","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB47271.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","02:45:00","MST",{"$nulls":4},147,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61902",81590,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6935194,-114.6203461,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999215164","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},147,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB47271.CHEM/results/999215164/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2024-01-09T09:20:59","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45171.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","01:38:00","MST",{"$nulls":4},36.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62868",82239,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2528438,-110.0338152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-974992816","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,36.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45171.CHEM/results/974992816/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-25T10:52:31","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45493.CHEM","Sample-Routine","Water","Groundwater","2023-03-29","02:21:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994694627","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,D1,.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45493.CHEM/results/994694627/resdetectqntlmts","Laboratory Reporting Level",20,"ug/L",{"$nulls":3},"2023-12-04T10:20:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48174.CHEM","Sample-Routine","Water","Groundwater","2023-01-30","01:40:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62060",81670,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6933939,-114.6214188,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992995337","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48174.CHEM/results/992995337/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2023-11-09T09:46:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48977.CHEM","Sample-Routine","Water","Groundwater","2023-01-17","02:18:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62776",82155,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.485781,-112.1016998,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993014730","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48977.CHEM/results/993014730/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49012.CHEM","Sample-Routine","Water","Groundwater","2023-03-30","12:23:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62484",81931,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947,-112.0021,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993019170","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49012.CHEM/results/993019170/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:01","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48192.CHEM","Sample-Routine","Water","Groundwater","2023-01-30","01:05:00","MST",{"$nulls":4},142,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55380",68281,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6932833,-114.6211361,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992996686","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},142,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48192.CHEM/results/992996686/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB44377.CHEM","Sample-Routine","Other","Groundwater","2023-02-10","02:54:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992962397","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB44377.CHEM/results/992962397/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:43:08","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49041.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","02:30:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62234",81738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4949968,-112.0012566,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993021316","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49041.CHEM/results/993021316/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49019.CHEM","Sample-Routine","Water","Groundwater","2023-03-28","10:35:00","MST",{"$nulls":4},92,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62235",81739,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4947199,-112.0021762,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993019688","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},92,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49019.CHEM/results/993019688/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:03","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46323.CHEM","Sample-Routine","Water","Groundwater","2023-03-23","10:40:00","MST",{"$nulls":4},164,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62562",81997,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4990217,-112.1466122,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992978667","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},164,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46323.CHEM/results/992978667/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:45:06","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48071.CHEM","Sample-Routine","Water","Groundwater","2023-01-25","03:45:00","MST",{"$nulls":4},160,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62554",81989,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945952,-114.6203669,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992994588","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},160,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48071.CHEM/results/992994588/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:46:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49447.CHEM","Sample-Routine","Water","Groundwater","2023-03-06","01:00:00","MST",{"$nulls":4},230,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-63154",82473,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5192115,-112.0806546,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993024280","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},230,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49447.CHEM/results/993024280/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:49:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50503.CHEM","Sample-Routine","Water","Groundwater","2023-06-02","09:28:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63071",82405,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0494496,-112.1508268,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706569","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,45,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50503.CHEM/results/994706569/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45534.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:49:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62860",82231,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.255927,-110.0234277,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083729","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45534.CHEM/results/975083729/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-30T10:53:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50512.CHEM","Sample-Routine","Water","Groundwater","2023-05-31","03:45:00","MST",{"$nulls":4},12,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47012",56624,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0477975,-112.1493457,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994707244","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,12,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50512.CHEM/results/994707244/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46004.CHEM","Sample-Routine","Other","Groundwater","2023-05-04","03:32:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992976365","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46004.CHEM/results/992976365/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:44:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46003.CHEM","Sample-Routine","Other","Groundwater","2023-05-04","02:43:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992976297","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46003.CHEM/results/992976297/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:44:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46354.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","09:48:00","MST",{"$nulls":4},93,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62952",82318,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3836634,-110.776152,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,93,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46354.CHEM/results/983662780/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49088.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","05:27:00","MST",{"$nulls":4},33,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62977",82343,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.335875,-110.9417802,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705004","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,33,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49088.CHEM/results/994705004/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49096.CHEM","Sample-Routine","Water","Groundwater","2023-06-08","08:34:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62988",82354,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.33581,-110.9417227,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705598","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49096.CHEM/results/994705598/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49097.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-07","04:26:00","MST",{"$nulls":4},32,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62989",82355,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359302,-110.9417269,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705672","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,32,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49097.CHEM/results/994705672/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:41","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50499.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","09:55:00","MST",{"$nulls":4},20,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63055",82389,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0487386,-112.1489839,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706269","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,20,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50499.CHEM/results/994706269/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46358.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","02:34:00","MST",{"$nulls":4},94,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62951",82317,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833447,-110.7755438,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983663076","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},94,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46358.CHEM/results/983663076/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46594.CHEM","Sample-Routine","Other","Groundwater","2023-05-10","10:56:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992983524","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46594.CHEM/results/992983524/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:45:34","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46344.CHEM","Sample-Routine","Water","Groundwater","2023-04-27","11:10:00","MST",{"$nulls":4},84,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62943",82309,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3834455,-110.7762108,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662034","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: M1,R5,.",null,84,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46344.CHEM/results/983662034/resdetectqntlmts","Laboratory Reporting Level",5.98,"ug/L",{"$nulls":3},"2023-07-26T11:00:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46347.CHEM","Sample-Routine","Water","Groundwater","2023-04-26","12:38:00","MST",{"$nulls":4},74,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62938",82304,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3833563,-110.7760749,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662257","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},74,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46347.CHEM/results/983662257/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:29","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48571.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","01:45:00","MST",{"$nulls":4},159,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-15970",24732,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6941992,-114.6281436,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993001343","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,159,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48571.CHEM/results/993001343/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49158.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","02:17:00","MST",{"$nulls":4},65,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-59153",80431,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1512278,-109.9755694,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016358","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},65,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49158.CHEM/results/993016358/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49161.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","12:47:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-43964",49738,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.149659,-109.972995,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993016580","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49161.CHEM/results/993016580/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46577.CHEM","Sample-Routine","Other","Groundwater","2023-05-11","04:45:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992982368","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46577.CHEM/results/992982368/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:45:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46222.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:20:00","MST",{"$nulls":4},98,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-54199",65608,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.5280103,-112.0834631,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992985027","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},98,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46222.CHEM/results/992985027/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:45:43","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49085.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","10:35:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62978",82344,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358918,-110.9416598,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704780","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49085.CHEM/results/994704780/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45529.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","03:14:00","MST",{"$nulls":4},30.5,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62862",82233,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.255957,-110.0239318,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083461","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,30.5,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45529.CHEM/results/975083461/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-30T10:53:26","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49086.CHEM","Sample-Routine","Water","Groundwater","2023-06-08","11:50:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62979",82345,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357929,-110.9418056,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704854","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49086.CHEM/results/994704854/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48987.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","12:37:00","MST",{"$nulls":4},305,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62775",82154,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4867908,-112.100564,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013990","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},305,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48987.CHEM/results/993013990/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50498.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","11:01:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47007",56619,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484,-112.148911,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706195","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50498.CHEM/results/994706195/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46345.CHEM","Sample-Routine","Water","Groundwater","2023-04-25","12:56:00","MST",{"$nulls":4},96,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62945",82311,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.383618,-110.7758978,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662109","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},96,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46345.CHEM/results/983662109/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:28","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50501.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","03:34:00","MST",{"$nulls":4},6,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63056",82390,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0484119,-112.1499339,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706421","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,6,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50501.CHEM/results/994706421/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48546.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","10:55:00","MST",{"$nulls":4},165,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61907",81595,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6943898,-114.6224328,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999760256","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R7.",null,165,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48546.CHEM/results/999760256/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2024-01-19T08:41:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50510.CHEM","Sample-Routine","Water","Groundwater","2023-06-01","08:45:00","MST",{"$nulls":4},18,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-47010",56622,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.048881,-112.1491475,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994707096","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,18,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50510.CHEM/results/994707096/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50506.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-02","11:37:00","MST",{"$nulls":4},17,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-63061",82395,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.0483203,-112.1490083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994706798","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8,H1,.",null,17,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50506.CHEM/results/994706798/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46309.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","10:55:00","MST",{"$nulls":4},195,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-55494",68499,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6945844,-114.6232625,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992979185","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},195,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46309.CHEM/results/992979185/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:45:09","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46310.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","10:05:00","MST",{"$nulls":4},136,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62057",81667,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6938676,-114.6203393,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-999651493","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: R5.",null,136,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46310.CHEM/results/999651493/resdetectqntlmts","Laboratory Reporting Level",2.99,"ug/L",{"$nulls":3},"2024-01-18T09:30:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49098.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-06-07","09:35:00","MST",{"$nulls":4},30,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62983",82349,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3357611,-110.9416976,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705747","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,30,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49098.CHEM/results/994705747/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:42","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48983.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","11:04:00","MST",{"$nulls":4},134,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62774",82153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4868778,-112.1006288,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013694","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},134,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48983.CHEM/results/993013694/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49087.CHEM","Sample-Routine","Water","Groundwater","2023-06-07","03:25:00","MST",{"$nulls":4},31,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62980",82346,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3356966,-110.9418481,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704928","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,31,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49087.CHEM/results/994704928/resdetectqntlmts","Laboratory Reporting Level",100,"ug/L",{"$nulls":3},"2023-12-04T10:21:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46352.CHEM","Sample-Routine","Water","Groundwater","2023-04-26","10:48:00","MST",{"$nulls":4},103,"ft",{"$nulls":5},9631,"2016-UNDERGROUND STORAGE TANKS","MATRIX NEW WORLD ENGINEERING, INC.","AZDEQ_WPD-62941",82307,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.3840379,-110.7762873,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-983662632","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},103,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46352.CHEM/results/983662632/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-07-26T11:00:32","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49082.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","02:56:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62985",82351,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3359064,-110.9418538,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994704551","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49082.CHEM/results/994704551/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48988.CHEM","Sample-Routine","Water","Groundwater","2023-04-14","11:25:00","MST",{"$nulls":4},141,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62774",82153,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.4868778,-112.1006288,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993014064","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},141,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48988.CHEM/results/993014064/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:35","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49092.CHEM","Sample-Routine","Water","Groundwater","2023-06-06","04:15:00","MST",{"$nulls":4},34,"ft",{"$nulls":5},9684,"2017-LEAKING UNDERGROUND STORAGE TANKS","STANTEC CONSULTING, INC.","AZDEQ_WPD-62984",82350,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},31.3358115,-110.9418872,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-994705300","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: E8.",null,34,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"EUROFINS ENVIRONMENT TESTING SOUTHWEST",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49092.CHEM/results/994705300/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-12-04T10:21:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48552.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","10:20:00","MST",{"$nulls":4},147,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-61904",81592,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6940346,-114.6214261,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992999924","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},147,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48552.CHEM/results/992999924/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:12","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB46604.CHEM","Sample-Routine","Other","Groundwater","2023-05-11","02:25:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-992984204","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB46604.CHEM/results/992984204/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:45:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48982.CHEM","Quality Control Sample-Field Replicate","Water","Groundwater","2023-04-14","12:00:00","MST",{"$nulls":4},150,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-62776",82155,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},33.485781,-112.1016998,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993013620","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},150,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48982.CHEM/results/993013620/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:33","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB48558.CHEM","Sample-Routine","Water","Groundwater","2023-04-04","09:50:00","MST",{"$nulls":4},115,"ft",{"$nulls":5},9749,"2018-WQARF Samples","MATRIX DESIGN GROUP INC / MATRIX ENVIRONMENTAL SERVICES, LLC","AZDEQ_WPD-62060",81670,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.6933939,-114.6214188,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993000372","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},115,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB48558.CHEM/results/993000372/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:47:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB49167.CHEM","Sample-Routine","Water","Groundwater","2023-04-05","12:05:00","MST",{"$nulls":4},155,"ft",{"$nulls":5},9749,"2018-WQARF Samples","Pinyon Environmental, Inc","AZDEQ_WPD-61930",81618,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.1544917,-109.9803722,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993017024","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},155,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB49167.CHEM/results/993017024/resdetectqntlmts","Laboratory Reporting Level",0.299,"ug/L",{"$nulls":3},"2023-11-09T09:48:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB45531.CHEM","Sample-Routine","Water","Groundwater","2023-05-03","02:34:00","MST",{"$nulls":4},28,"ft",{"$nulls":5},9651,"2016-LEAKING UNDERGROUND STORAGE TANKS","Terranext, LLC.","AZDEQ_WPD-62859",82230,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.2558122,-110.0239078,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-975083571","Not Detected",null,"1,3-Butadiene","Total",{"$nulls":3},"Final",null,"Estimated",{"$nulls":9},"| QA FLAGS: T4.",null,28,"ft",{"$nulls":6},"EPA 8260B","AZDEQ_WPD","EPA 8260B",null,null,"Orange Coast Analytical, Inc.",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB45531.CHEM/results/975083571/resdetectqntlmts","Laboratory Reporting Level",10,"ug/L",{"$nulls":3},"2023-05-30T10:53:27","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50985.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","12:41:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035265","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50985.CHEM/results/993035265/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51525.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","11:17:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52476",62766,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2259808,-110.9666858,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038566","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51525.CHEM/results/993038566/resdetectqntlmts","Laboratory Reporting Level",0.0443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50984.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","09:31:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035197","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50984.CHEM/results/993035197/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51002.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:55:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036421","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51002.CHEM/results/993036421/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50996.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","12:05:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036013","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50996.CHEM/results/993036013/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50980.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","08:33:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034925","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50980.CHEM/results/993034925/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50893.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","10:36:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63479",82795,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9009139,-110.1588167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034449","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50893.CHEM/results/993034449/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50992.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","04:09:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035741","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50992.CHEM/results/993035741/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51533.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","01:10:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52475",62765,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258156,-110.9669394,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993039110","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51533.CHEM/results/993039110/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51531.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","09:28:00","MST",{"$nulls":4},45,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63545",82856,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2259876,-110.9667495,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038974","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},45,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51531.CHEM/results/993038974/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50993.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","10:42:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62324",81825,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035809","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50993.CHEM/results/993035809/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50888.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","02:59:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034109","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50888.CHEM/results/993034109/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50988.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","12:43:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62338",81835,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035469","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50988.CHEM/results/993035469/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50983.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:01:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62333",81830,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035129","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50983.CHEM/results/993035129/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50987.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","10:51:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62322",81823,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035401","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50987.CHEM/results/993035401/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50986.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:44:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035333","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50986.CHEM/results/993035333/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:19","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50978.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","11:45:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034789","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50978.CHEM/results/993034789/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50974.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","03:33:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62314",81815,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034517","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50974.CHEM/results/993034517/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50982.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:57:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62340",81837,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035061","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50982.CHEM/results/993035061/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:18","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50995.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:57:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035945","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50995.CHEM/results/993035945/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51004.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","04:25:00","MST",{"$nulls":4},13.7,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62317",81818,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036557","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},13.7,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51004.CHEM/results/993036557/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50889.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","01:43:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63480",82796,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9007889,-110.1590667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034177","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50889.CHEM/results/993034177/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51529.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","12:21:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63546",82857,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258496,-110.9666718,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038838","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51529.CHEM/results/993038838/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51001.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","10:46:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036353","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51001.CHEM/results/993036353/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51527.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","03:35:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52474",62764,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258108,-110.9664744,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038702","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51527.CHEM/results/993038702/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50981.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","02:33:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034993","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50981.CHEM/results/993034993/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50998.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","11:14:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036149","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50998.CHEM/results/993036149/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50994.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","02:13:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035877","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50994.CHEM/results/993035877/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:22","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50976.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","12:10:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62337",81834,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034653","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50976.CHEM/results/993034653/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50891.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","02:38:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034313","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50891.CHEM/results/993034313/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51528.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:38:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63547",82858,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2260778,-110.9664476,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038770","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51528.CHEM/results/993038770/resdetectqntlmts","Laboratory Reporting Level",0.0443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:37","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51530.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:57:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63544",82855,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2258612,-110.9668172,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038906","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51530.CHEM/results/993038906/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:38","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50989.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:42:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035537","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50989.CHEM/results/993035537/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:20","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50890.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","04:23:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034245","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50890.CHEM/results/993034245/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50991.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:32:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035673","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50991.CHEM/results/993035673/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51005.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","12:20:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036625","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51005.CHEM/results/993036625/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51526.CHEM","Sample-Routine","Other","Groundwater","2023-09-26","01:24:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-52473",62763,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2262686,-110.9664731,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993038634","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51526.CHEM/results/993038634/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:36","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50997.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","10:13:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62311",81812,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232588,-110.972266,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036081","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50997.CHEM/results/993036081/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51532.CHEM","Sample-Routine","Other","Groundwater","2023-09-25","11:18:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63543",82854,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2260615,-110.9666247,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993039042","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51532.CHEM/results/993039042/resdetectqntlmts","Laboratory Reporting Level",0.443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:39","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50979.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","01:03:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034857","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50979.CHEM/results/993034857/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:17","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50999.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","02:50:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036217","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50999.CHEM/results/993036217/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:23","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51003.CHEM","Sample-Routine","Other","Groundwater","2023-08-22","11:24:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036489","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51003.CHEM/results/993036489/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:25","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50977.CHEM","Sample-Routine","Other","Groundwater","2023-08-23","02:01:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62342",81839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034721","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50977.CHEM/results/993034721/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:16","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50975.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","03:49:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62315",81816,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034585","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50975.CHEM/results/993034585/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50892.CHEM","Sample-Routine","Other","Groundwater","2023-08-18","03:35:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-63478",82794,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9005639,-110.1590444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993034381","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50892.CHEM/results/993034381/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB50990.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","12:22:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62318",81819,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993035605","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB50990.CHEM/results/993035605/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:21","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB51000.CHEM","Sample-Routine","Other","Groundwater","2023-08-21","11:17:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},9725,"2017-WQARF SAMPLES","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-993036285","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB51000.CHEM/results/993036285/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-11-09T09:50:24","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52416.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:03:00","MST",{"$nulls":4},40,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62325",81826,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361574","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},40,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52416.CHEM/results/997361574/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52440.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","10:56:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62332",81829,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363206","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52440.CHEM/results/997363206/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52430.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:10:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62336",81833,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362526","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52430.CHEM/results/997362526/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52347.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","03:48:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63481",82797,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006333,-110.1591111,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323972","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52347.CHEM/results/997323972/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52415.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","01:36:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62320",81821,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361506","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52415.CHEM/results/997361506/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52417.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:09:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62333",81830,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361642","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52417.CHEM/results/997361642/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52343.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","05:25:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63479",82795,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9009139,-110.1588167,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323700","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52343.CHEM/results/997323700/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52345.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","03:14:00","MST",{"$nulls":4},9,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63482",82798,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006833,-110.159225,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323836","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52345.CHEM/results/997323836/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52427.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:38:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62338",81835,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362322","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52427.CHEM/results/997362322/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52439.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:12:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62341",81838,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363138","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52439.CHEM/results/997363138/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52432.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:36:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62318",81819,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362662","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52432.CHEM/results/997362662/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52433.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:24:00","MST",{"$nulls":4},60,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62326",81827,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362730","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},60,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52433.CHEM/results/997362730/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52436.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:44:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62342",81839,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362934","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52436.CHEM/results/997362934/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52344.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","04:51:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63477",82793,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9006417,-110.1589778,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323768","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52344.CHEM/results/997323768/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:13","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52420.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:59:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62335",81832,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361846","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52420.CHEM/results/997361846/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52434.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","11:46:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62334",81831,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2328028,-110.9722306,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362798","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52434.CHEM/results/997362798/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:51","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52437.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:28:00","MST",{"$nulls":4},85,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62337",81834,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2327056,-110.9721917,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363002","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},85,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52437.CHEM/results/997363002/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52414.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:16:00","MST",{"$nulls":4},13.7,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62317",81818,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361438","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},13.7,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52414.CHEM/results/997361438/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52418.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:40:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62315",81816,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361710","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52418.CHEM/results/997361710/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:46","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52422.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:52:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62319",81820,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.23271,-110.972855,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361982","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52422.CHEM/results/997361982/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52426.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","12:54:00","MST",{"$nulls":4},36,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62339",81836,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326056,-110.9722861,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362254","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},36,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52426.CHEM/results/997362254/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52441.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:23:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62314",81815,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232497,-110.972199,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363274","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52441.CHEM/results/997363274/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52348.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","02:48:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63480",82796,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9007889,-110.1590667,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997324040","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52348.CHEM/results/997324040/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:15","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52429.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","10:49:00","MST",{"$nulls":4},5.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62312",81813,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362458","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52429.CHEM/results/997362458/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52435.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","11:30:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62311",81812,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232588,-110.972266,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362866","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52435.CHEM/results/997362866/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:52","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52428.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","01:12:00","MST",{"$nulls":4},11,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62323",81824,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362390","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},11,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52428.CHEM/results/997362390/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52425.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","10:30:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62308",81809,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232809,-110.972298,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362186","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52425.CHEM/results/997362186/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:49","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52411.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","11:13:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62309",81810,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232801,-110.972185,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361234","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52411.CHEM/results/997361234/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:44","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52412.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:03:00","MST",{"$nulls":4},7.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62316",81817,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232498,-110.972333,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361302","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},7.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52412.CHEM/results/997361302/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52438.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","12:56:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62322",81823,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232994,-110.972292,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363070","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52438.CHEM/results/997363070/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:53","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52346.CHEM","Sample-Routine","Other","Groundwater","2023-12-01","04:22:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10093,"WQARF-513132","HYDRO GEO CHEM","AZDEQ_WPD-63478",82794,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},34.9005639,-110.1590444,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997323904","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52346.CHEM/results/997323904/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-28T09:24:14","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52442.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","01:31:00","MST",{"$nulls":4},21,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62340",81837,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997363342","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},21,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52442.CHEM/results/997363342/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:54","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52424.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","02:01:00","MST",{"$nulls":4},9.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62321",81822,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232989,-110.972568,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362118","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},9.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52424.CHEM/results/997362118/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:48","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52419.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","01:46:00","MST",{"$nulls":4},72,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62327",81828,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361778","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},72,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52419.CHEM/results/997361778/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52413.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","10:50:00","MST",{"$nulls":4},5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62310",81811,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232617,-110.972087,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361370","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52413.CHEM/results/997361370/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:45","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52431.CHEM","Sample-Routine","Other","Groundwater","2023-11-10","02:02:00","MST",{"$nulls":4},86,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62343",81840,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.2326861,-110.9724472,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362594","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},86,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52431.CHEM/results/997362594/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:50","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52421.CHEM","Sample-Routine","Other","Groundwater","2023-11-08","11:08:00","MST",{"$nulls":4},14.5,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62313",81814,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232496,-110.972083,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997361914","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},14.5,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52421.CHEM/results/997361914/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:47","STORET"]
["AZDEQ_WPD","AZDEQ_WPD","AZDEQ_WPD-AB52423.CHEM","Sample-Routine","Other","Groundwater","2023-11-09","12:40:00","MST",{"$nulls":4},15,"ft",{"$nulls":5},10117,"WQARF-512567","HYDRO GEO CHEM","AZDEQ_WPD-62324",81825,"--- SAMPLE TAKEN: Yes; Normal Flow",{"$nulls":3},32.232693,-110.972207,"Unknown","AZDEQ_WPD","Unknown",null,"Miscellaneous (Other)","STORET-997362050","Not Detected",null,"1,3-Butadiene","Total Recoverable",{"$nulls":3},"Final",null,"Estimated",{"$nulls":11},15,"ft",{"$nulls":6},"METHOD TO-15","AZDEQ_WPD","METHOD TO-15",null,null,"PACE ANALYTICAL CENTER FOR TESTING AND INNOVATION",null,null,"https://www.waterqualitydata.us/data/providers/STORET/organizations/AZDEQ_WPD/activities/AZDEQ_WPD-AB52423.CHEM/results/997362050/resdetectqntlmts","Laboratory Reporting Level",0.00443,"mg/m3",{"$nulls":3},"2023-12-29T09:53:48","STORET"]
[]
[{"$nulls":77},"mean",{"$f":"AVERAGE(CA4657:CA4681)","v":6.8848}]
[{"$nulls":77},"median",{"$f":"MEDIAN(CA4657:CA4681)","v":2.6}]