Running script REVS_config_ambient_load ...
Running ambient=class_REVS_ambient; 

Running script REVS_config_vehicle_load ...
Running vehicle_PS 
Loading vehicle_PS
Running PS_driver 
Loading PS_driver

Running script REVS_config_engine_load ...
Running engine_2018_Toyota_A25AFKS_2L5_Tier3 

Running script REVS_config_transmission_load ...
Running PS_transmission_ECVT 
Loading PS_transmission_ECVT

Running script REVS_config_electric_load ...
Running PS_electric 
Loading PS_electric
Loading battery_base_Samsung_LI_Power_mod2 
Running emachine_2010_Toyota_Prius_60kW_650V_MG1_EMOT 
Running emachine_2010_Toyota_Prius_60kW_650V_MG2_EMOT 

Running script REVS_config_accessories_load ...
Running PS_accessories 
Loading PS_accessories

Running script REVS_config_engine_modify ...

Running script REVS_config_transmission_modify ...

Running script REVS_config_electric_modify ...

Running script REVS_config_vehicle_modify ...

Running script PS_preprocess ...

Running script REVS_config_external_data_modify ...

Running script REVS_config_HVM_controls_load ...
Running PS_controls 
Loading PS_controls

Running script REVS_config_HVM_controls_update ...

[Warning: The System object 'PS_control' in MATLAB System block '<a href="matlab:open_and_hilite_hyperlink ('REVS_VM/powertrain/PS Hybrid/controls/HVM control PS/MATLAB System','error')">REVS_VM/powertrain/PS Hybrid/controls/HVM control PS/MATLAB System</a>' declares the property 'engine_start_time' as a Discrete
State, but does not use it in the stepImpl or outputImpl methods. Simulink will not log this property and will suppress it in the generated code.] 
### Building the Accelerator target for model: REVS_VM
### Generating code into build folder: /Users/kevinnewman/Code/GitHub/ALPHA_REVS3/ALPHA_DEMO/output/ALPHA_PS_DEMO_sim/slprj/accel/REVS_VM
### Serializing module
### Writing machine code
### Successfully built the Accelerator target for model: REVS_VM

Running REVS_postprocess_DCDC_log
Running REVS_postprocess_accessory_battery_log
Running REVS_postprocess_alternator_log
Running REVS_postprocess_drive_motor_log
Running REVS_postprocess_engine_basics_log
Running REVS_postprocess_engine_idle_log
Running REVS_postprocess_mech_accessories_log
Running REVS_postprocess_propulsion_battery_log
Running REVS_postprocess_transmission_log
Running REVS_postprocess_vehicle_basics_log
Running REVS_postprocess_vehicle_performance_log

       ---------- Phase Results ----------
   EPA_UDDS_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.607 mi
   Fuel Consumption            = 206.4006 grams
   Fuel Consumption            = 0.0734 gallons
   Fuel Economy (Volumetric)   = 49.171 mpg
   Fuel Consumption            = 57.220 g/mile
   CO2 Emission                = 174.00 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   4.02 kWh/100mi
   Energy Consumption          = 144.87 Wh
   Energy Efficiency           =     40 Wh/mi

   EPA_UDDS_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.887 mi
   Fuel Consumption            = 259.3134 grams
   Fuel Consumption            = 0.0922 gallons
   Fuel Economy (Volumetric)   = 42.173 mpg
   Fuel Consumption            = 66.714 g/mile
   CO2 Emission                = 202.87 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   0.47 kWh/100mi
   Energy Consumption          =  18.25 Wh
   Energy Efficiency           =      5 Wh/mi

   EPA_HWFET: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.267 mi
   Fuel Consumption            = 565.2871 grams
   Fuel Consumption            = 0.2009 gallons
   Fuel Economy (Volumetric)   = 51.101 mpg
   Fuel Consumption            = 55.059 g/mile
   CO2 Emission                = 167.43 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   1.19 kWh/100mi
   Energy Consumption          = 122.14 Wh
   Energy Efficiency           =     12 Wh/mi

   EPA_US06_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  1.787 mi
   Fuel Consumption            = 147.3596 grams
   Fuel Consumption            = 0.0524 gallons
   Fuel Economy (Volumetric)   = 34.116 mpg
   Fuel Consumption            = 82.469 g/mile
   CO2 Emission                = 250.78 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           = -12.84 kWh/100mi
   Energy Consumption          = -229.48 Wh
   Energy Efficiency           =   -128 Wh/mi

   EPA_US06_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  6.245 mi
   Fuel Consumption            = 433.0815 grams
   Fuel Consumption            = 0.1539 gallons
   Fuel Economy (Volumetric)   = 40.570 mpg
   Fuel Consumption            = 69.350 g/mile
   CO2 Emission                = 210.89 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   1.98 kWh/100mi
   Energy Consumption          = 123.87 Wh
   Energy Efficiency           =     20 Wh/mi

       --------- Weighted Results --------
   EPA_UDDS: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  7.494 mi
   Fuel Consumption            = 465.7140 grams
   Fuel Consumption            = 0.1655 gallons
   Fuel Economy (Volumetric)   = 45.274 mpg
   Fuel Consumption            = 62.144 g/mile
   CO2 Emission                = 188.98 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   2.18 kWh/100mi
   Energy Consumption          = 163.12 Wh
   Energy Efficiency           =     22 Wh/mi

   EPA_HWFET: ----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.267 mi
   Fuel Consumption            = 565.2871 grams
   Fuel Consumption            = 0.2009 gallons
   Fuel Economy (Volumetric)   = 51.101 mpg
   Fuel Consumption            = 55.059 g/mile
   CO2 Emission                = 167.43 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   1.19 kWh/100mi
   Energy Consumption          = 122.14 Wh
   Energy Efficiency           =     12 Wh/mi

   EPA_US06: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  8.032 mi
   Fuel Consumption            = 580.4410 grams
   Fuel Consumption            = 0.2063 gallons
   Fuel Economy (Volumetric)   = 38.932 mpg
   Fuel Consumption            = 72.268 g/mile
   CO2 Emission                = 219.76 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -1.31 kWh/100mi
   Energy Consumption          = -105.61 Wh
   Energy Efficiency           =    -13 Wh/mi

   EPA_UDDS_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  7610.61 kJ
    Fuel Energy                  =  7042.61 kJ     92.54%
    Stored Energy                =   568.00 kJ      7.46%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2809.18 kJ
    Engine Energy                =  2287.66 kJ   81.44%
         Engine Efficiency       =    32.48 %
    Stored Energy                =   521.52 kJ     18.56%
        Propulsion Batt. Energy  =   521.52 kJ     18.56%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1634.51 kJ     58.18%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   103.29 kJ      3.68%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   102.03 kJ      3.63%
         Electrical              =   102.03 kJ      3.63%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     1.19 kJ      0.04%
    Battery Stored Charge        =     0.06 kJ      0.00%
    Total Electrical Accessories =   102.03 kJ      3.63%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1071.48 kJ     38.14%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =    24.57 kJ      0.87%
     Driveline Emachines         =   952.93 kJ     33.92%
         MG1                     =   302.47 kJ     10.77%
         MG2                     =   650.45 kJ     23.15%
     Gearbox                     =    68.38 kJ      2.43%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =     0.00 kJ      0.00%
         Gear Loss               =    68.38 kJ      2.43%
         Inertia Loss            =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    13.31 kJ      0.47%
     Tire Slip                   =    12.30 kJ      0.44%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2809.28 kJ
Simulation Error                 =    -0.10 kJ
Energy Conservation              =  100.004 %

   EPA_UDDS_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 10775.80 kJ
    Fuel Energy                  = 10675.55 kJ     99.07%
    Stored Energy                =   100.25 kJ      0.93%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2755.93 kJ
    Engine Energy                =  2690.22 kJ   97.62%
         Engine Efficiency       =    25.20 %
    Stored Energy                =    65.71 kJ      2.38%
        Propulsion Batt. Energy  =    65.71 kJ      2.38%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1154.51 kJ     41.89%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   181.25 kJ      6.58%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   172.86 kJ      6.27%
         Electrical              =   172.86 kJ      6.27%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     1.62 kJ      0.06%
    Battery Stored Charge        =     6.78 kJ      0.25%
    Total Electrical Accessories =   172.86 kJ      6.27%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1418.82 kJ     51.48%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =    14.55 kJ      0.53%
     Driveline Emachines         =  1303.92 kJ     47.31%
         MG1                     =   476.28 kJ     17.28%
         MG2                     =   827.64 kJ     30.03%
     Gearbox                     =    59.25 kJ      2.15%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =     0.00 kJ      0.00%
         Gear Loss               =    59.25 kJ      2.15%
         Inertia Loss            =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    28.43 kJ      1.03%
     Tire Slip                   =    12.67 kJ      0.46%
System Kinetic Energy Gain       =     1.41 kJ      0.05%
                                    ------------
Total Loss Energy                =  2755.99 kJ
Simulation Error                 =    -0.07 kJ
Energy Conservation              =  100.002 %

   EPA_HWFET audit: ----------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 22990.37 kJ
    Fuel Energy                  = 22528.87 kJ     97.99%
    Stored Energy                =   461.50 kJ      2.01%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  8358.81 kJ
    Engine Energy                =  7919.11 kJ   94.74%
         Engine Efficiency       =    35.15 %
    Stored Energy                =   439.70 kJ      5.26%
        Propulsion Batt. Energy  =   439.70 kJ      5.26%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  6015.38 kJ     71.96%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   159.16 kJ      1.90%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   153.05 kJ      1.83%
         Electrical              =   153.05 kJ      1.83%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     1.38 kJ      0.02%
    Battery Stored Charge        =     4.73 kJ      0.06%
    Total Electrical Accessories =   153.05 kJ      1.83%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  2184.22 kJ     26.13%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =    14.45 kJ      0.17%
     Driveline Emachines         =  2002.91 kJ     23.96%
         MG1                     =   648.80 kJ      7.76%
         MG2                     =  1354.11 kJ     16.20%
     Gearbox                     =   152.66 kJ      1.83%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =     0.00 kJ      0.00%
         Gear Loss               =   152.66 kJ      1.83%
         Inertia Loss            =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =     1.98 kJ      0.02%
     Tire Slip                   =    12.22 kJ      0.15%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  8358.77 kJ
Simulation Error                 =     0.04 kJ
Energy Conservation              =  100.000 %

   EPA_US06_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  8412.91 kJ
    Fuel Energy                  =  8412.91 kJ    100.00%
    Stored Energy                =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2837.50 kJ
    Engine Energy                =  2837.50 kJ  100.00%
         Engine Efficiency       =    33.73 %
    Stored Energy                =     0.00 kJ      0.00%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =   949.85 kJ     33.48%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =    49.04 kJ      1.73%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =    47.01 kJ      1.66%
         Electrical              =    47.01 kJ      1.66%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     0.83 kJ      0.03%
    Battery Stored Charge        =     1.20 kJ      0.04%
    Total Electrical Accessories =    47.01 kJ      1.66%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1838.58 kJ     64.80%
     Battery Stored Charge       =   826.14 kJ     29.12%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =    36.59 kJ      1.29%
     Driveline Emachines         =   611.29 kJ     21.54%
         MG1                     =   222.14 kJ      7.83%
         MG2                     =   389.15 kJ     13.71%
     Gearbox                     =    75.52 kJ      2.66%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =     0.00 kJ      0.00%
         Gear Loss               =    75.52 kJ      2.66%
         Inertia Loss            =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   260.61 kJ      9.18%
     Tire Slip                   =    28.43 kJ      1.00%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2837.46 kJ
Simulation Error                 =     0.04 kJ
Energy Conservation              =   99.999 %

   EPA_US06_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 17444.26 kJ
    Fuel Energy                  = 16965.47 kJ     97.26%
    Stored Energy                =   478.79 kJ      2.74%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  6731.41 kJ
    Engine Energy                =  6285.47 kJ   93.38%
         Engine Efficiency       =    37.05 %
    Stored Energy                =   445.94 kJ      6.62%
        Propulsion Batt. Energy  =   445.94 kJ      6.62%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  5207.59 kJ     77.36%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =    75.73 kJ      1.13%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =    73.02 kJ      1.08%
         Electrical              =    73.02 kJ      1.08%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     0.87 kJ      0.01%
    Battery Stored Charge        =     1.84 kJ      0.03%
    Total Electrical Accessories =    73.02 kJ      1.08%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1447.89 kJ     21.51%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =    25.47 kJ      0.38%
     Driveline Emachines         =  1239.95 kJ     18.42%
         MG1                     =   396.09 kJ      5.88%
         MG2                     =   843.86 kJ     12.54%
     Gearbox                     =   113.29 kJ      1.68%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =     0.00 kJ      0.00%
         Gear Loss               =   113.29 kJ      1.68%
         Inertia Loss            =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    51.62 kJ      0.77%
     Tire Slip                   =    17.57 kJ      0.26%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  6731.20 kJ
Simulation Error                 =     0.21 kJ
Energy Conservation              =   99.997 %

   EPA_UDDS & EPA_HWFET & EPA_US06 audit: 

         ---- Energy Audit Report ----

Gross Energy Provided            = 66455.88 kJ
    Fuel Energy                  = 65625.47 kJ     98.75%
    Stored Energy                =   830.41 kJ      1.25%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              = 22666.70 kJ
    Engine Energy                = 22019.96 kJ   97.15%
         Engine Efficiency       =    33.55 %
    Stored Energy                =   646.74 kJ      2.85%
        Propulsion Batt. Energy  =   646.74 kJ      2.85%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  = 14961.84 kJ     66.01%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   568.48 kJ      2.51%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   547.98 kJ      2.42%
         Electrical              =   547.98 kJ      2.42%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     5.89 kJ      0.03%
    Battery Stored Charge        =    14.61 kJ      0.06%
    Total Electrical Accessories =   547.98 kJ      2.42%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  7134.85 kJ     31.48%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =   115.62 kJ      0.51%
     Driveline Emachines         =  6111.00 kJ     26.96%
         MG1                     =  2045.78 kJ      9.03%
         MG2                     =  4065.22 kJ     17.93%
     Gearbox                     =   469.09 kJ      2.07%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =     0.00 kJ      0.00%
         Gear Loss               =   469.09 kJ      2.07%
         Inertia Loss            =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   355.95 kJ      1.57%
     Tire Slip                   =    83.19 kJ      0.37%
System Kinetic Energy Gain       =     1.41 kJ      0.01%
                                    ------------
Total Loss Energy                = 22666.58 kJ
Simulation Error                 =     0.12 kJ
Energy Conservation              =   99.999 %

