Running script REVS_config_ambient_load ...
Running ambient=class_REVS_ambient; 

Running script REVS_config_vehicle_load ...
Running vehicle_P2 
Loading vehicle_P2
Running P2_driver 
Loading P2_driver

Running script REVS_config_engine_load ...
Running engine_2018_Toyota_A25AFKS_2L5_Tier3 

Running script REVS_config_transmission_load ...
Running TRX12_FWD_P2_Hybrid 
Loading TRX12_FWD_P2_Hybrid

Running script REVS_config_electric_load ...
Running P2_electric 
Loading P2_electric
Running emachine_2012_Hyundai_Sonata_8p5kW_270V_BISG 
Running emachine_2011_Hyundai_Sonata_30kW_270V_EMOT 
Loading battery_9p8_kWh_NCM 

Running script REVS_config_accessories_load ...
Running P2_accessories 
Loading P2_accessories

Running script REVS_config_engine_modify ...

Running script REVS_config_transmission_modify ...

Running script REVS_config_electric_modify ...

Running script REVS_config_vehicle_modify ...

Running script CVM_P0_P2_preprocess ...
ans =
          628.318530717959

Running script REVS_config_external_data_modify ...

Running script REVS_config_HVM_controls_load ...
Running P2_controls 
Loading P2_controls

Running script REVS_config_HVM_controls_update ...


Running REVS_postprocess_DCDC_log
Running REVS_postprocess_accessory_battery_log
Running REVS_postprocess_alternator_log
Running REVS_postprocess_drive_motor_log
Running REVS_postprocess_engine_basics_log
Running REVS_postprocess_engine_idle_log
Running REVS_postprocess_mech_accessories_log
Running REVS_postprocess_propulsion_battery_log
Running REVS_postprocess_transmission_log
Running REVS_postprocess_vehicle_basics_log
Running REVS_postprocess_vehicle_performance_log

       ---------- Phase Results ----------
   EPA_UDDS_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.604 mi
   Fuel Consumption            = 187.8267 grams
   Fuel Consumption            = 0.0668 gallons
   Fuel Economy (Volumetric)   = 53.992 mpg
   Fuel Consumption            = 52.110 g/mile
   CO2 Emission                = 158.46 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   0.23 kWh/100mi
   Energy Consumption          =   8.12 Wh
   Energy Efficiency           =      2 Wh/mi

   EPA_UDDS_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.883 mi
   Fuel Consumption            = 201.1916 grams
   Fuel Consumption            = 0.0715 gallons
   Fuel Economy (Volumetric)   = 54.295 mpg
   Fuel Consumption            = 51.819 g/mile
   CO2 Emission                = 157.58 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   3.49 kWh/100mi
   Energy Consumption          = 135.57 Wh
   Energy Efficiency           =     35 Wh/mi

   EPA_HWFET: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.263 mi
   Fuel Consumption            = 541.3691 grams
   Fuel Consumption            = 0.1924 gallons
   Fuel Economy (Volumetric)   = 53.338 mpg
   Fuel Consumption            = 52.749 g/mile
   CO2 Emission                = 160.41 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.33 kWh/100mi
   Energy Consumption          = -34.33 Wh
   Energy Efficiency           =     -3 Wh/mi

   EPA_US06_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  1.788 mi
   Fuel Consumption            = 133.8127 grams
   Fuel Consumption            = 0.0476 gallons
   Fuel Economy (Volumetric)   = 37.595 mpg
   Fuel Consumption            = 74.839 g/mile
   CO2 Emission                = 227.58 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -7.37 kWh/100mi
   Energy Consumption          = -131.86 Wh
   Energy Efficiency           =    -74 Wh/mi

   EPA_US06_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  6.242 mi
   Fuel Consumption            = 434.5375 grams
   Fuel Consumption            = 0.1544 gallons
   Fuel Economy (Volumetric)   = 40.418 mpg
   Fuel Consumption            = 69.611 g/mile
   CO2 Emission                = 211.68 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.30 kWh/100mi
   Energy Consumption          = -18.64 Wh
   Energy Efficiency           =     -3 Wh/mi

       --------- Weighted Results --------
   EPA_UDDS: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  7.487 mi
   Fuel Consumption            = 389.0182 grams
   Fuel Consumption            = 0.1383 gallons
   Fuel Economy (Volumetric)   = 54.149 mpg
   Fuel Consumption            = 51.959 g/mile
   CO2 Emission                = 158.00 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   1.92 kWh/100mi
   Energy Consumption          = 143.69 Wh
   Energy Efficiency           =     19 Wh/mi

   EPA_HWFET: ----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.263 mi
   Fuel Consumption            = 541.3691 grams
   Fuel Consumption            = 0.1924 gallons
   Fuel Economy (Volumetric)   = 53.338 mpg
   Fuel Consumption            = 52.749 g/mile
   CO2 Emission                = 160.41 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.33 kWh/100mi
   Energy Consumption          = -34.33 Wh
   Energy Efficiency           =     -3 Wh/mi

   EPA_US06: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  8.030 mi
   Fuel Consumption            = 568.3502 grams
   Fuel Consumption            = 0.2020 gallons
   Fuel Economy (Volumetric)   = 39.753 mpg
   Fuel Consumption            = 70.775 g/mile
   CO2 Emission                = 215.22 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -1.87 kWh/100mi
   Energy Consumption          = -150.50 Wh
   Energy Efficiency           =    -19 Wh/mi

   EPA_UDDS_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  7880.09 kJ
    Fuel Energy                  =  7789.49 kJ     98.85%
    Stored Energy                =    90.60 kJ      1.15%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2985.15 kJ
    Engine Energy                =  2946.86 kJ   98.72%
         Engine Efficiency       =    37.83 %
    Stored Energy                =    38.29 kJ      1.28%
        Propulsion Batt. Energy  =    29.22 kJ      0.98%
        Accessory Batt. Energy   =     9.07 kJ      0.30%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1631.94 kJ     54.66%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   263.46 kJ      8.82%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   255.36 kJ      8.55%
         Electrical              =   255.36 kJ      8.55%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     8.10 kJ      0.27%
    Battery Stored Charge        =     0.00 kJ      0.00%
    Total Electrical Accessories =   255.36 kJ      8.55%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1090.45 kJ     36.52%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.01 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =    14.27 kJ      0.48%
     P0 Gearing             =     3.92 kJ      0.13%
     P2 Motor Generator     =   761.76 kJ     25.51%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   238.47 kJ      7.99%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =   101.92 kJ      3.41%
         Gear Loss               =   117.57 kJ      3.94%
         Inertia Loss            =    18.98 kJ      0.64%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    59.08 kJ      1.98%
     Tire Slip                   =    12.94 kJ      0.43%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2985.85 kJ
Simulation Error                 =    -0.70 kJ
Energy Conservation              =  100.024 %

   EPA_UDDS_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  7465.70 kJ
    Fuel Energy                  =  6927.85 kJ     92.80%
    Stored Energy                =   537.84 kJ      7.20%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  3064.68 kJ
    Engine Energy                =  2576.63 kJ   84.08%
         Engine Efficiency       =    37.19 %
    Stored Energy                =   488.04 kJ     15.92%
        Propulsion Batt. Energy  =   488.04 kJ     15.92%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1152.53 kJ     37.59%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   450.22 kJ     14.69%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   432.65 kJ     14.11%
         Electrical              =   432.65 kJ     14.11%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    14.20 kJ      0.46%
    Battery Stored Charge        =     3.37 kJ      0.11%
    Total Electrical Accessories =   432.65 kJ     14.11%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1463.08 kJ     47.72%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.01 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =    13.90 kJ      0.45%
     P0 Gearing             =     3.39 kJ      0.11%
     P2 Motor Generator     =  1099.50 kJ     35.86%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   248.65 kJ      8.11%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =    90.11 kJ      2.94%
         Gear Loss               =   126.24 kJ      4.12%
         Inertia Loss            =    32.30 kJ      1.05%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    84.16 kJ      2.74%
     Tire Slip                   =    13.48 kJ      0.44%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  3065.83 kJ
Simulation Error                 =    -1.15 kJ
Energy Conservation              =  100.038 %

   EPA_HWFET audit: ----------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 23098.78 kJ
    Fuel Energy                  = 23046.32 kJ     99.77%
    Stored Energy                =    52.46 kJ      0.23%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  8932.06 kJ
    Engine Energy                =  8932.06 kJ  100.00%
         Engine Efficiency       =    38.76 %
    Stored Energy                =     0.00 kJ      0.00%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  6010.37 kJ     67.29%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   397.98 kJ      4.46%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   383.07 kJ      4.29%
         Electrical              =   383.07 kJ      4.29%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    12.55 kJ      0.14%
    Battery Stored Charge        =     2.35 kJ      0.03%
    Total Electrical Accessories =   383.07 kJ      4.29%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  2523.82 kJ     28.26%
     Battery Stored Charge       =   123.60 kJ      1.38%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.01 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =    14.11 kJ      0.16%
     P0 Gearing             =     3.94 kJ      0.04%
     P2 Motor Generator     =  1703.54 kJ     19.07%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   570.50 kJ      6.39%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =   335.39 kJ      3.75%
         Gear Loss               =   230.86 kJ      2.58%
         Inertia Loss            =     4.26 kJ      0.05%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    95.71 kJ      1.07%
     Tire Slip                   =    12.41 kJ      0.14%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  8932.17 kJ
Simulation Error                 =    -0.11 kJ
Energy Conservation              =  100.001 %

   EPA_US06_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  6895.63 kJ
    Fuel Energy                  =  6895.63 kJ    100.00%
    Stored Energy                =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2553.54 kJ
    Engine Energy                =  2553.54 kJ  100.00%
         Engine Efficiency       =    37.03 %
    Stored Energy                =     0.00 kJ      0.00%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =   952.21 kJ     37.26%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   122.12 kJ      4.78%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   117.67 kJ      4.60%
         Electrical              =   117.67 kJ      4.60%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     3.85 kJ      0.15%
    Battery Stored Charge        =     0.59 kJ      0.02%
    Total Electrical Accessories =   117.67 kJ      4.60%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1481.08 kJ     57.96%
     Battery Stored Charge       =   474.68 kJ     18.58%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.07 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =    20.10 kJ      0.79%
     P0 Gearing             =     6.34 kJ      0.25%
     P2 Motor Generator     =   561.68 kJ     21.98%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   214.04 kJ      8.38%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =    69.30 kJ      2.71%
         Gear Loss               =   109.56 kJ      4.29%
         Inertia Loss            =    35.18 kJ      1.38%
     Final Drive                 =    -0.00 kJ     -0.00%
     Friction Brakes             =   172.68 kJ      6.76%
     Tire Slip                   =    31.49 kJ      1.23%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2555.41 kJ
Simulation Error                 =    -1.87 kJ
Energy Conservation              =  100.073 %

   EPA_US06_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 18476.94 kJ
    Fuel Energy                  = 18411.81 kJ     99.65%
    Stored Energy                =    65.14 kJ      0.35%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  7082.65 kJ
    Engine Energy                =  7082.65 kJ  100.00%
         Engine Efficiency       =    38.47 %
    Stored Energy                =     0.00 kJ      0.00%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  5201.85 kJ     73.44%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   189.67 kJ      2.68%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   182.77 kJ      2.58%
         Electrical              =   182.77 kJ      2.58%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     5.98 kJ      0.08%
    Battery Stored Charge        =     0.91 kJ      0.01%
    Total Electrical Accessories =   182.77 kJ      2.58%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1691.40 kJ     23.88%
     Battery Stored Charge       =    67.12 kJ      0.95%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.01 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =    18.26 kJ      0.26%
     P0 Gearing             =     6.53 kJ      0.09%
     P2 Motor Generator     =   981.96 kJ     13.86%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   505.08 kJ      7.13%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =   300.17 kJ      4.24%
         Gear Loss               =   196.83 kJ      2.78%
         Inertia Loss            =     8.07 kJ      0.11%
     Final Drive                 =    -0.00 kJ     -0.00%
     Friction Brakes             =    93.30 kJ      1.32%
     Tire Slip                   =    19.15 kJ      0.27%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  7082.92 kJ
Simulation Error                 =    -0.26 kJ
Energy Conservation              =  100.004 %

   EPA_UDDS & EPA_HWFET & EPA_US06 audit: 

         ---- Energy Audit Report ----

Gross Energy Provided            = 63430.76 kJ
    Fuel Energy                  = 63071.09 kJ     99.43%
    Stored Energy                =   359.67 kJ      0.57%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              = 24093.58 kJ
    Engine Energy                = 24091.74 kJ   99.99%
         Engine Efficiency       =    38.20 %
    Stored Energy                =     1.84 kJ      0.01%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     1.84 kJ      0.01%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  = 14948.90 kJ     62.03%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =  1416.22 kJ      5.88%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =  1371.54 kJ      5.69%
         Electrical              =  1371.54 kJ      5.69%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    44.68 kJ      0.19%
    Battery Stored Charge        =     0.00 kJ      0.00%
    Total Electrical Accessories =  1371.54 kJ      5.69%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  7732.56 kJ     32.09%
     Battery Stored Charge       =   148.13 kJ      0.61%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.10 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     Driveline Emachines         =     0.00 kJ      0.00%
     P0 Motor Generator     =    80.64 kJ      0.33%
     P0 Gearing             =    24.12 kJ      0.10%
     P2 Motor Generator     =  5108.44 kJ     21.20%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =  1776.73 kJ      7.37%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =   896.89 kJ      3.72%
         Gear Loss               =   781.05 kJ      3.24%
         Inertia Loss            =    98.79 kJ      0.41%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   504.92 kJ      2.10%
     Tire Slip                   =    89.47 kJ      0.37%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                = 24097.69 kJ
Simulation Error                 =    -4.10 kJ
Energy Conservation              =  100.017 %

