Running script REVS_config_ambient_load ...
Running ambient=class_REVS_ambient; 

Running script REVS_config_vehicle_load ...
Running vehicle_CVM_P0 
Loading vehicle_CVM_P0
Running CVM_P0_driver 
Loading CVM_P0_driver

Running script REVS_config_engine_load ...
Running engine_2018_Toyota_A25AFKS_2L5_Tier3 

Running script REVS_config_transmission_load ...
Running transmission_6AT_FWD_midsize_car 
Loading transmission_6AT_FWD_midsize_car

Running script REVS_config_electric_load ...
Running P0_electric 
Loading P0_electric
Running emachine_2012_Hyundai_Sonata_8p5kW_270V_BISG 
Running P0_battery_pack 
Loading P0_battery_pack

Running script REVS_config_accessories_load ...
Running accessory_EPS_param 
Loading accessory_EPS_param

Running script REVS_config_CVM_controls_load ...
Running P0_controls 
Loading P0_controls

Running script REVS_config_engine_modify ...

Running script REVS_config_transmission_modify ...

Running script REVS_config_electric_modify ...

Running script REVS_config_vehicle_modify ...

Running script CVM_P0_P2_preprocess ...

Running script REVS_config_external_data_modify ...

Running script REVS_config_CVM_controls_update ...

### Building the Accelerator target for model: REVS_VM
### Generating code into build folder: /Users/kevinnewman/Code/GitHub/ALPHA_REVS3/ALPHA_DEMO/output/ALPHA_P0_DEMO_sim/slprj/accel/REVS_VM
### Serializing module
### Writing machine code
### Successfully built the Accelerator target for model: REVS_VM

Running REVS_postprocess_DCDC_log
Running REVS_postprocess_accessory_battery_log
Running REVS_postprocess_alternator_log
Running REVS_postprocess_drive_motor_log
Running REVS_postprocess_engine_basics_log
Running REVS_postprocess_engine_idle_log
Running REVS_postprocess_mech_accessories_log
Running REVS_postprocess_propulsion_battery_log
Running REVS_postprocess_transmission_log
Running REVS_postprocess_vehicle_basics_log
Running REVS_postprocess_vehicle_performance_log

       ---------- Phase Results ----------
   EPA_UDDS_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.611 mi
   Fuel Consumption            = 239.0698 grams
   Fuel Consumption            = 0.0850 gallons
   Fuel Economy (Volumetric)   = 42.501 mpg
   Fuel Consumption            = 66.200 g/mile
   CO2 Emission                = 201.31 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.37 kWh/100mi
   Energy Consumption          = -13.41 Wh
   Energy Efficiency           =     -4 Wh/mi

   EPA_UDDS_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.888 mi
   Fuel Consumption            = 293.3790 grams
   Fuel Consumption            = 0.1043 gallons
   Fuel Economy (Volumetric)   = 37.283 mpg
   Fuel Consumption            = 75.464 g/mile
   CO2 Emission                = 229.48 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   0.28 kWh/100mi
   Energy Consumption          =  11.01 Wh
   Energy Efficiency           =      3 Wh/mi

   EPA_HWFET: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.269 mi
   Fuel Consumption            = 575.7545 grams
   Fuel Consumption            = 0.2046 gallons
   Fuel Economy (Volumetric)   = 50.180 mpg
   Fuel Consumption            = 56.069 g/mile
   CO2 Emission                = 170.50 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.23 kWh/100mi
   Energy Consumption          = -23.91 Wh
   Energy Efficiency           =     -2 Wh/mi

   EPA_US06_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  1.796 mi
   Fuel Consumption            = 215.3843 grams
   Fuel Consumption            = 0.0766 gallons
   Fuel Economy (Volumetric)   = 23.467 mpg
   Fuel Consumption            = 119.894 g/mile
   CO2 Emission                = 364.59 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -3.45 kWh/100mi
   Energy Consumption          = -62.04 Wh
   Energy Efficiency           =    -35 Wh/mi

   EPA_US06_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  6.245 mi
   Fuel Consumption            = 473.3364 grams
   Fuel Consumption            = 0.1682 gallons
   Fuel Economy (Volumetric)   = 37.124 mpg
   Fuel Consumption            = 75.789 g/mile
   CO2 Emission                = 230.47 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =   0.25 kWh/100mi
   Energy Consumption          =  15.46 Wh
   Energy Efficiency           =      2 Wh/mi

       --------- Weighted Results --------
   EPA_UDDS: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  7.499 mi
   Fuel Consumption            = 532.4488 grams
   Fuel Consumption            = 0.1892 gallons
   Fuel Economy (Volumetric)   = 39.626 mpg
   Fuel Consumption            = 71.003 g/mile
   CO2 Emission                = 215.91 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.03 kWh/100mi
   Energy Consumption          =  -2.39 Wh
   Energy Efficiency           =     -0 Wh/mi

   EPA_HWFET: ----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.269 mi
   Fuel Consumption            = 575.7545 grams
   Fuel Consumption            = 0.2046 gallons
   Fuel Economy (Volumetric)   = 50.180 mpg
   Fuel Consumption            = 56.069 g/mile
   CO2 Emission                = 170.50 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.23 kWh/100mi
   Energy Consumption          = -23.91 Wh
   Energy Efficiency           =     -2 Wh/mi

   EPA_US06: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  8.042 mi
   Fuel Consumption            = 688.7208 grams
   Fuel Consumption            = 0.2448 gallons
   Fuel Economy (Volumetric)   = 32.853 mpg
   Fuel Consumption            = 85.641 g/mile
   CO2 Emission                = 260.43 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  -0.58 kWh/100mi
   Energy Consumption          = -46.58 Wh
   Energy Efficiency           =     -6 Wh/mi

   EPA_UDDS_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 10187.61 kJ
    Fuel Energy                  = 10179.55 kJ     99.92%
    Stored Energy                =     8.07 kJ      0.08%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  3012.00 kJ
    Engine Energy                =  3004.82 kJ   99.76%
         Engine Efficiency       =    29.52 %
    Stored Energy                =     7.18 kJ      0.24%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     7.18 kJ      0.24%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1636.23 kJ     54.32%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   205.47 kJ      6.82%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   199.09 kJ      6.61%
         Electrical              =   199.09 kJ      6.61%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     6.38 kJ      0.21%
    Battery Stored Charge        =     0.00 kJ      0.00%
    Total Electrical Accessories =   199.09 kJ      6.61%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1170.75 kJ     38.86%
     Battery Stored Charge       =    48.26 kJ      1.60%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =   135.55 kJ      4.50%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =   189.16 kJ      6.28%
     P0 Gearing             =    73.06 kJ      2.43%
     Gearbox                     =   600.94 kJ     19.95%
         Pump Loss               =   290.79 kJ      9.65%
         Spin Loss               =   162.04 kJ      5.38%
         Gear Loss               =   130.14 kJ      4.32%
         Inertia Loss            =    17.97 kJ      0.60%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   110.90 kJ      3.68%
     Tire Slip                   =    12.87 kJ      0.43%
System Kinetic Energy Gain       =     0.02 kJ      0.00%
                                    ------------
Total Loss Energy                =  3012.47 kJ
Simulation Error                 =    -0.47 kJ
Energy Conservation              =  100.016 %

   EPA_UDDS_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 12250.23 kJ
    Fuel Energy                  = 12185.54 kJ     99.47%
    Stored Energy                =    64.68 kJ      0.53%
    Kinetic Energy               =     0.02 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  3015.42 kJ
    Engine Energy                =  2975.76 kJ   98.68%
         Engine Efficiency       =    24.42 %
    Stored Energy                =    39.64 kJ      1.31%
        Propulsion Batt. Energy  =    39.64 kJ      1.31%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.02 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1154.36 kJ     38.27%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   351.05 kJ     11.64%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   337.32 kJ     11.18%
         Electrical              =   337.32 kJ     11.18%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    11.11 kJ      0.37%
    Battery Stored Charge        =     2.62 kJ      0.09%
    Total Electrical Accessories =   337.32 kJ     11.18%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1510.74 kJ     50.09%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =   218.53 kJ      7.25%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =   185.88 kJ      6.16%
     P0 Gearing             =    70.82 kJ      2.35%
     Gearbox                     =   816.81 kJ     27.08%
         Pump Loss               =   458.56 kJ     15.20%
         Spin Loss               =   179.03 kJ      5.94%
         Gear Loss               =   151.49 kJ      5.02%
         Inertia Loss            =    27.74 kJ      0.92%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   205.56 kJ      6.82%
     Tire Slip                   =    13.15 kJ      0.44%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  3016.15 kJ
Simulation Error                 =    -0.73 kJ
Energy Conservation              =  100.024 %

   EPA_HWFET audit: ----------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 24387.63 kJ
    Fuel Energy                  = 24387.63 kJ    100.00%
    Stored Energy                =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  8119.78 kJ
    Engine Energy                =  8119.78 kJ  100.00%
         Engine Efficiency       =    33.29 %
    Stored Energy                =     0.00 kJ      0.00%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  6015.98 kJ     74.09%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   310.32 kJ      3.82%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   298.66 kJ      3.68%
         Electrical              =   298.66 kJ      3.68%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     9.82 kJ      0.12%
    Battery Stored Charge        =     1.83 kJ      0.02%
    Total Electrical Accessories =   298.66 kJ      3.68%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1793.67 kJ     22.09%
     Battery Stored Charge       =    86.08 kJ      1.06%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =   138.40 kJ      1.70%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =   140.51 kJ      1.73%
     P0 Gearing             =    65.82 kJ      0.81%
     Gearbox                     =  1261.43 kJ     15.53%
         Pump Loss               =   551.09 kJ      6.79%
         Spin Loss               =   450.15 kJ      5.54%
         Gear Loss               =   250.41 kJ      3.08%
         Inertia Loss            =     9.79 kJ      0.12%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    88.94 kJ      1.10%
     Tire Slip                   =    12.48 kJ      0.15%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  8119.97 kJ
Simulation Error                 =    -0.18 kJ
Energy Conservation              =  100.002 %

   EPA_US06_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  9639.30 kJ
    Fuel Energy                  =  9639.30 kJ    100.00%
    Stored Energy                =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2952.07 kJ
    Engine Energy                =  2952.07 kJ  100.00%
         Engine Efficiency       =    30.63 %
    Stored Energy                =     0.00 kJ      0.00%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =   956.98 kJ     32.39%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =    95.22 kJ      3.22%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =    91.74 kJ      3.10%
         Electrical              =    91.74 kJ      3.10%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     3.01 kJ      0.10%
    Battery Stored Charge        =     0.46 kJ      0.02%
    Total Electrical Accessories =    91.74 kJ      3.10%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1902.65 kJ     64.39%
     Battery Stored Charge       =   223.36 kJ      7.56%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =   186.98 kJ      6.33%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =   225.01 kJ      7.61%
     P0 Gearing             =   100.77 kJ      3.41%
     Gearbox                     =   532.01 kJ     18.00%
         Pump Loss               =   186.66 kJ      6.32%
         Spin Loss               =   158.34 kJ      5.36%
         Gear Loss               =   112.96 kJ      3.82%
         Inertia Loss            =    74.05 kJ      2.51%
     Final Drive                 =    -0.00 kJ     -0.00%
     Friction Brakes             =   603.45 kJ     20.42%
     Tire Slip                   =    31.07 kJ      1.05%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2954.85 kJ
Simulation Error                 =    -2.78 kJ
Energy Conservation              =  100.094 %

   EPA_US06_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            = 19799.21 kJ
    Fuel Energy                  = 19708.06 kJ     99.54%
    Stored Energy                =    91.15 kJ      0.46%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  6814.95 kJ
    Engine Energy                =  6759.28 kJ   99.18%
         Engine Efficiency       =    34.30 %
    Stored Energy                =    55.67 kJ      0.82%
        Propulsion Batt. Energy  =    55.67 kJ      0.82%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  5204.53 kJ     76.36%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   147.89 kJ      2.17%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   142.50 kJ      2.09%
         Electrical              =   142.50 kJ      2.09%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     4.68 kJ      0.07%
    Battery Stored Charge        =     0.71 kJ      0.01%
    Total Electrical Accessories =   142.50 kJ      2.09%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1463.73 kJ     21.47%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =   136.00 kJ      2.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =   128.77 kJ      1.89%
     P0 Gearing             =    54.40 kJ      0.80%
     Gearbox                     =   981.36 kJ     14.40%
         Pump Loss               =   338.58 kJ      4.97%
         Spin Loss               =   398.03 kJ      5.84%
         Gear Loss               =   195.25 kJ      2.86%
         Inertia Loss            =    49.50 kJ      0.73%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   143.91 kJ      2.11%
     Tire Slip                   =    19.29 kJ      0.28%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  6816.16 kJ
Simulation Error                 =    -1.21 kJ
Energy Conservation              =  100.018 %

   EPA_UDDS & EPA_HWFET & EPA_US06 audit: 

         ---- Energy Audit Report ----

Gross Energy Provided            = 76104.28 kJ
    Fuel Energy                  = 76100.07 kJ     99.99%
    Stored Energy                =     4.20 kJ      0.01%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              = 23813.27 kJ
    Engine Energy                = 23811.71 kJ   99.99%
         Engine Efficiency       =    31.29 %
    Stored Energy                =     1.55 kJ      0.01%
        Propulsion Batt. Energy  =     0.00 kJ      0.00%
        Accessory Batt. Energy   =     1.55 kJ      0.01%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  = 14968.09 kJ     62.84%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =  1104.33 kJ      4.64%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =  1069.32 kJ      4.49%
         Electrical              =  1069.32 kJ      4.49%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    35.01 kJ      0.15%
    Battery Stored Charge        =     0.00 kJ      0.00%
    Total Electrical Accessories =  1069.32 kJ      4.49%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  7746.23 kJ     32.52%
     Battery Stored Charge       =   262.39 kJ      1.10%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =   815.46 kJ      3.42%
     High Voltage DCDC           =     0.00 kJ      0.00%
     Driveline Emachines         =     0.00 kJ      0.00%
     P0 Motor Generator     =   869.34 kJ      3.65%
     P0 Gearing             =   364.86 kJ      1.53%
     Gearbox                     =  4192.55 kJ     17.60%
         Pump Loss               =  1825.67 kJ      7.66%
         Spin Loss               =  1347.59 kJ      5.66%
         Gear Loss               =   840.24 kJ      3.53%
         Inertia Loss            =   179.04 kJ      0.75%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =  1152.76 kJ      4.84%
     Tire Slip                   =    88.87 kJ      0.37%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                = 23818.65 kJ
Simulation Error                 =    -5.38 kJ
Energy Conservation              =  100.023 %

