Running script REVS_config_ambient_load ...
Running ambient=class_REVS_ambient; 

Running script REVS_config_vehicle_load ...
Running vehicle_P2 
Loading vehicle_P2
Running P2_driver 
Loading P2_driver

Running script REVS_config_engine_load ...
Running engine_2018_Toyota_A25AFKS_2L5_Tier3 

Running script REVS_config_transmission_load ...
Running TRX12_FWD_P2_Hybrid 
Loading TRX12_FWD_P2_Hybrid

Running script REVS_config_electric_load ...
Running P2_electric 
Loading P2_electric
Running emachine_2012_Hyundai_Sonata_8p5kW_270V_BISG 
Running emachine_2011_Hyundai_Sonata_30kW_270V_EMOT 
Loading battery_9p8_kWh_NCM 

Running script REVS_config_accessories_load ...
Running P2_accessories 
Loading P2_accessories

Running script REVS_config_engine_modify ...

Running script REVS_config_transmission_modify ...

Running script REVS_config_electric_modify ...

Running script REVS_config_vehicle_modify ...

Running script CVM_P0_P2_preprocess ...
ans =
          628.318530717959

Running script REVS_config_external_data_modify ...

Running script REVS_config_HVM_controls_load ...
Running P2_controls 
Loading P2_controls

Running script REVS_config_HVM_controls_update ...

### Building the Accelerator target for model: REVS_VM
### Generating code into build folder: /Users/kevinnewman/Code/GitHub/ALPHA_REVS3/ALPHA_DEMO/output/ALPHA_P2_PHEV_DEMO_sim/slprj/accel/REVS_VM
### Serializing module
### Writing machine code
### Successfully built the Accelerator target for model: REVS_VM

Running REVS_postprocess_DCDC_log
Running REVS_postprocess_accessory_battery_log
Running REVS_postprocess_alternator_log
Running REVS_postprocess_drive_motor_log
Running REVS_postprocess_engine_basics_log
Running REVS_postprocess_engine_idle_log
Running REVS_postprocess_mech_accessories_log
Running REVS_postprocess_propulsion_battery_log
Running REVS_postprocess_transmission_log
Running REVS_postprocess_vehicle_basics_log
Running REVS_postprocess_vehicle_performance_log

       ---------- Phase Results ----------
   EPA_UDDS_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.604 mi
   Fuel Consumption            =    NaN grams
   Fuel Consumption            =    NaN gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                =    NaN g/mile

   Energy Economy              = 133.35 MPGe
   Energy Efficiency           =  22.75 kWh/100mi
   Energy Consumption          = 819.92 Wh
   Energy Efficiency           =    227 Wh/mi

   EPA_UDDS_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.883 mi
   Fuel Consumption            =    NaN grams
   Fuel Consumption            =    NaN gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                =    NaN g/mile

   Energy Economy              = 141.35 MPGe
   Energy Efficiency           =  21.46 kWh/100mi
   Energy Consumption          = 833.25 Wh
   Energy Efficiency           =    215 Wh/mi

   EPA_HWFET: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.263 mi
   Fuel Consumption            =    NaN grams
   Fuel Consumption            =    NaN gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                =    NaN g/mile

   Energy Economy              = 129.97 MPGe
   Energy Efficiency           =  23.34 kWh/100mi
   Energy Consumption          = 2395.31 Wh
   Energy Efficiency           =    233 Wh/mi

   EPA_US06_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  1.788 mi
   Fuel Consumption            =    NaN grams
   Fuel Consumption            =    NaN gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                =    NaN g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  27.59 kWh/100mi
   Energy Consumption          = 493.16 Wh
   Energy Efficiency           =    276 Wh/mi

   EPA_US06_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  6.242 mi
   Fuel Consumption            =    NaN grams
   Fuel Consumption            =    NaN gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                =    NaN g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  28.40 kWh/100mi
   Energy Consumption          = 1772.91 Wh
   Energy Efficiency           =    284 Wh/mi

       --------- Weighted Results --------
   EPA_UDDS: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  7.487 mi
   Fuel Consumption            = 439.7511 grams
   Fuel Consumption            = 0.1563 gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                = 178.61 g/mile

   Energy Economy              = 137.38 MPGe
   Energy Efficiency           =  22.08 kWh/100mi
   Energy Consumption          = 1653.16 Wh
   Energy Efficiency           =    221 Wh/mi

   EPA_HWFET: ----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.263 mi
   Fuel Consumption            = 554.9516 grams
   Fuel Consumption            = 0.1972 gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                = 164.43 g/mile

   Energy Economy              = 129.97 MPGe
   Energy Efficiency           =  23.34 kWh/100mi
   Energy Consumption          = 2395.31 Wh
   Energy Efficiency           =    233 Wh/mi

   EPA_US06: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  8.030 mi
   Fuel Consumption            = 588.5518 grams
   Fuel Consumption            = 0.2092 gallons
   Fuel Economy (Volumetric)   =    NaN mpg
   Fuel Consumption            =    NaN g/mile
   CO2 Emission                = 222.88 g/mile

   Energy Economy              =    NaN MPGe
   Energy Efficiency           =  28.22 kWh/100mi
   Energy Consumption          = 2266.07 Wh
   Energy Efficiency           =    282 Wh/mi

   EPA_UDDS_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  3011.80 kJ
    Fuel Energy                  =     0.00 kJ      0.00%
    Stored Energy                =  3011.80 kJ    100.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2960.77 kJ
    Engine Energy                =     0.00 kJ    0.00%
         Engine Efficiency       =      NaN %
    Stored Energy                =  2960.77 kJ    100.00%
        Propulsion Batt. Energy  =  2951.70 kJ     99.69%
        Accessory Batt. Energy   =     9.07 kJ      0.31%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1631.90 kJ     55.11%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   263.46 kJ      8.90%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   255.36 kJ      8.62%
         Electrical              =   255.36 kJ      8.62%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     8.10 kJ      0.27%
    Battery Stored Charge        =     0.00 kJ      0.00%
    Total Electrical Accessories =   255.36 kJ      8.62%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1065.66 kJ     35.99%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =    -0.00 kJ     -0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =     0.00 kJ      0.00%
     P0 Gearing             =     0.00 kJ      0.00%
     P2 Motor Generator     =   772.39 kJ     26.09%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   221.74 kJ      7.49%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =    87.66 kJ      2.96%
         Gear Loss               =   115.67 kJ      3.91%
         Inertia Loss            =    18.41 kJ      0.62%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    59.10 kJ      2.00%
     Tire Slip                   =    12.44 kJ      0.42%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2961.03 kJ
Simulation Error                 =    -0.26 kJ
Energy Conservation              =  100.009 %

   EPA_UDDS_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  3032.44 kJ
    Fuel Energy                  =     0.00 kJ      0.00%
    Stored Energy                =  3032.44 kJ    100.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2999.69 kJ
    Engine Energy                =     0.00 kJ    0.00%
         Engine Efficiency       =      NaN %
    Stored Energy                =  2999.69 kJ    100.00%
        Propulsion Batt. Energy  =  2999.69 kJ    100.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  1152.51 kJ     38.42%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   450.22 kJ     15.01%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   432.65 kJ     14.42%
         Electrical              =   432.65 kJ     14.42%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    14.20 kJ      0.47%
    Battery Stored Charge        =     3.37 kJ      0.11%
    Total Electrical Accessories =   432.65 kJ     14.42%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1397.39 kJ     46.58%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =    -0.00 kJ     -0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =     0.00 kJ      0.00%
     P0 Gearing             =     0.00 kJ      0.00%
     P2 Motor Generator     =  1066.95 kJ     35.56%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   233.83 kJ      7.79%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =    77.84 kJ      2.59%
         Gear Loss               =   123.96 kJ      4.13%
         Inertia Loss            =    32.03 kJ      1.07%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    83.85 kJ      2.79%
     Tire Slip                   =    12.76 kJ      0.43%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  3000.11 kJ
Simulation Error                 =    -0.42 kJ
Energy Conservation              =  100.014 %

   EPA_HWFET audit: ----------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  8725.00 kJ
    Fuel Energy                  =     0.00 kJ      0.00%
    Stored Energy                =  8725.00 kJ    100.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  8623.13 kJ
    Engine Energy                =     0.00 kJ    0.00%
         Engine Efficiency       =      NaN %
    Stored Energy                =  8623.13 kJ    100.00%
        Propulsion Batt. Energy  =  8623.13 kJ    100.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  6010.36 kJ     69.70%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   397.98 kJ      4.62%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   383.07 kJ      4.44%
         Electrical              =   383.07 kJ      4.44%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    12.55 kJ      0.15%
    Battery Stored Charge        =     2.35 kJ      0.03%
    Total Electrical Accessories =   383.07 kJ      4.44%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  2214.85 kJ     25.68%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =    -0.00 kJ     -0.00%
     Launch Device / Clutches    =     0.00 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =     0.00 kJ      0.00%
     P0 Gearing             =     0.00 kJ      0.00%
     P2 Motor Generator     =  1566.34 kJ     18.16%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   540.22 kJ      6.26%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =   305.55 kJ      3.54%
         Gear Loss               =   230.45 kJ      2.67%
         Inertia Loss            =     4.21 kJ      0.05%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    95.98 kJ      1.11%
     Tire Slip                   =    12.30 kJ      0.14%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  8623.19 kJ
Simulation Error                 =    -0.06 kJ
Energy Conservation              =  100.001 %

   EPA_US06_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  2749.29 kJ
    Fuel Energy                  =   886.11 kJ     32.23%
    Stored Energy                =  1863.19 kJ     67.77%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2080.87 kJ
    Engine Energy                =   305.49 kJ   14.68%
         Engine Efficiency       =    34.48 %
    Stored Energy                =  1775.37 kJ     85.32%
        Propulsion Batt. Energy  =  1775.37 kJ     85.32%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =   951.84 kJ     45.73%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   122.12 kJ      5.87%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   117.67 kJ      5.65%
         Electrical              =   117.67 kJ      5.65%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     3.85 kJ      0.19%
    Battery Stored Charge        =     0.59 kJ      0.03%
    Total Electrical Accessories =   117.67 kJ      5.65%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1007.26 kJ     48.40%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.01 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =     9.32 kJ      0.45%
     P0 Gearing             =     3.33 kJ      0.16%
     P2 Motor Generator     =   572.02 kJ     27.48%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   221.24 kJ     10.63%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =    59.38 kJ      2.85%
         Gear Loss               =   127.57 kJ      6.13%
         Inertia Loss            =    34.30 kJ      1.65%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   172.04 kJ      8.27%
     Tire Slip                   =    29.30 kJ      1.41%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2081.22 kJ
Simulation Error                 =    -0.36 kJ
Energy Conservation              =  100.017 %

   EPA_US06_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Provided            =  8310.10 kJ
    Fuel Energy                  =  1779.81 kJ     21.42%
    Stored Energy                =  6530.29 kJ     78.58%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  6996.48 kJ
    Engine Energy                =   614.01 kJ    8.78%
         Engine Efficiency       =    34.50 %
    Stored Energy                =  6382.47 kJ     91.22%
        Propulsion Batt. Energy  =  6382.47 kJ     91.22%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  =  5201.82 kJ     74.35%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   189.67 kJ      2.71%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   182.77 kJ      2.61%
         Electrical              =   182.77 kJ      2.61%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     5.98 kJ      0.09%
    Battery Stored Charge        =     0.91 kJ      0.01%
    Total Electrical Accessories =   182.77 kJ      2.61%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  1604.81 kJ     22.94%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.02 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     P0 Motor Generator     =    21.26 kJ      0.30%
     P0 Gearing             =     8.02 kJ      0.11%
     P2 Motor Generator     =   989.11 kJ     14.14%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =   473.49 kJ      6.77%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =   277.84 kJ      3.97%
         Gear Loss               =   190.10 kJ      2.72%
         Inertia Loss            =     5.55 kJ      0.08%
     Final Drive                 =    -0.00 kJ     -0.00%
     Friction Brakes             =    94.23 kJ      1.35%
     Tire Slip                   =    18.68 kJ      0.27%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  6996.30 kJ
Simulation Error                 =     0.18 kJ
Energy Conservation              =   99.997 %

   EPA_UDDS & EPA_HWFET & EPA_US06 audit: 

         ---- Energy Audit Report ----

Gross Energy Provided            = 25823.68 kJ
    Fuel Energy                  =  2665.92 kJ     10.32%
    Stored Energy                = 23157.76 kJ     89.68%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              = 23653.72 kJ
    Engine Energy                =   919.51 kJ    3.89%
         Engine Efficiency       =    34.49 %
    Stored Energy                = 22734.21 kJ     96.11%
        Propulsion Batt. Energy  = 22732.37 kJ     96.10%
        Accessory Batt. Energy   =     1.84 kJ      0.01%
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Energy Consumed by ABC roadload  = 14948.43 kJ     63.19%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =  1416.22 kJ      5.99%
    Starter                      =     0.00 kJ      0.00%
    Alternator                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =  1371.54 kJ      5.80%
         Electrical              =  1371.54 kJ      5.80%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    44.68 kJ      0.19%
    Battery Stored Charge        =     0.00 kJ      0.00%
    Total Electrical Accessories =  1371.54 kJ      5.80%
    Total Mechanical Accessories =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  7289.97 kJ     30.82%
     Battery Stored Charge       =     0.00 kJ      0.00%
     Engine                      =     0.00 kJ      0.00%
     Launch Device / Clutches    =     0.03 kJ      0.00%
     High Voltage DCDC           =     0.00 kJ      0.00%
     Driveline Emachines         =     0.00 kJ      0.00%
     P0 Motor Generator     =    30.58 kJ      0.13%
     P0 Gearing             =    11.36 kJ      0.05%
     P2 Motor Generator     =  4966.81 kJ     21.00%
     P2 Gearing             =     0.00 kJ      0.00%
     Gearbox                     =  1690.52 kJ      7.15%
         Pump Loss               =     0.00 kJ      0.00%
         Spin Loss               =   808.27 kJ      3.42%
         Gear Loss               =   787.75 kJ      3.33%
         Inertia Loss            =    94.50 kJ      0.40%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   505.19 kJ      2.14%
     Tire Slip                   =    85.48 kJ      0.36%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                = 23654.63 kJ
Simulation Error                 =    -0.91 kJ
Energy Conservation              =  100.004 %

