{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":8,"rows_kept":16}
[]
["Source Category","Emission Reduction Measure Name","Control Efficiency (%)*","SCCs To which Emission Reduction Measure Applies","Cost Effectiveness \n(2006$/ton)**","Other Pollutants Controlled","Description/Notes/Caveats","References"]
["Fireplaces","Use EPA Phase 2 Qualified Units",70,2104008100,"$9,500 **","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
[{"$nulls":7},"http://www.epa.gov/burnwise/resources.html"]
["Fireplaces","Use Gas Logs in Existing Wood-burning Fireplaces",99,2104008100,11000,"CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Fireplaces","Install Retrofit Devices into Wood-burning Fireplaces",70,2104008100,9500,"CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
[" Hydronic Heaters (OWHH, OWB)","Replace Uncertified Hydronic Heaters with Cleaner Burning Appliances ","up to 90",2104008610,"TBD","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Wood Burning Furnaces","Replace Uncertified Wood Burning Furnaces with Cleaner EPA Certified Wood Burning Furnaces ","up to 90","2104008510","TBD","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Wood Stoves","Wood to Wood Replacement Program","60-80",2104008310,"$9,900 (2010$)","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Wood Stoves","Wood to Gas Replacement Program",99,2104008310,"$7,200 (2010$)","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Wood Stoves","Remove Old Wood Stoves for Money or \"Bounty\"",70,2104008310,"$5,330/ton (2012$)","CO2, VOC's,CO CH4, Toxics, BC","Implement an incentive program (usually voluntary) where cash (e.g., $250) is given in return for turning in a wood stove. ","http://www.epa.gov/burnwise/resources.html"]
["Fireplaces, Hydronic Heaters, Wood Stoves","Curtailment Program       ( \"Burn Ban\")",75,"2104008100, 2104008310, 2104008610","$8,700 (2010$)","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Fireplaces, Hydronic Heaters, Wood Stoves","Burn Dry Seasoned Wood","n/a","2104008100, 2104008310, 2104008320, 2104008330, 2104008400, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC","Implement a program to only allow the sale of  and/or  burning of dry seasoned wood (e.g., <20% moisture content) in wood-burning appliances.  ","http://www.epa.gov/burnwise/resources.html"]
["Fireplaces, Hydronic Heaters, Wood Stoves","No visible Emissions","n/a","2104008100, 2104008310, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Fireplaces, Hydronic Heaters, Wood Stoves","Opacity Program","n/a","2104008100, 2104008310, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]
["Wood Combustion Appliances","Education Campaign","n/a","2104008100, 2104008310, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC",null,"http://www.epa.gov/burnwise/resources.html"]

{"sheet":"Sheet2","index":1,"n_rows":14,"n_cols":7,"rows_kept":14}
["Source Category","Emission Reduction Measure Name","Control Efficiency (%)*","SCCs To which Emission Reduction Measure Applies","Cost Effectiveness \n(2006$/ton)**","Other Pollutants Controlled","Description/Notes/Caveats"]
["Fireplaces","Use EPA Phase 2 Qualified Units",70,2104008100,"$9,500 **","CO2, VOC's,CO CH4, Toxics, BC","If new fireplace construction is allowed, approve only EPA Phase 2 qualified models.  Under the EPA Wood-burning Fireplace Program, cleaner wood-burning fireplaces are qualified when their PM2.5 emissions are at or below the Phase 2 PM2.5 emissions level. For a list of Phase 2 qualified cleaner burning fireplaces, go to: http://www.epa.gov/burnwise/fireplacelist.html. "]
["Fireplaces","Use Gas Logs in Existing Wood-burning Fireplaces",100,2104008100,{"v":11000,"d":"$11,000"},"CO2, VOC's,CO CH4, Toxics, BC"]
["Fireplaces","Install Retrofit Devices into Wood-burning Fireplaces",70,2104008100,{"v":9500,"d":"$9,500"},"CO2, VOC's,CO CH4, Toxics, BC"]
[" Hydronic Heaters (OWHH, OWB)","Replace Uncertified Hydronic Heaters with Cleaner EPA Certified Hydronic Heaters ",90,2104008610,"TBD","CO2, VOC's,CO CH4, Toxics, BC"]
["Wood Burning Furnaces","Replace Uncertified Wood Burning Furnaces with Cleaner EPA Certified Wood Burning Furnaces ",null,"2104008510","TBD","CO2, VOC's,CO CH4, Toxics, BC"]
["Wood Stoves","Wood to Wood Replacement Program",60,2104008310,"$9,900 (2010$)","CO2, VOC's,CO CH4, Toxics, BC"]
["Wood Stoves","Wood to Gas Replacement Program",99,2104008310,"$7,200 (2010$)","CO2, VOC's,CO CH4, Toxics, BC"]
["Wood Stoves","Remove Old Wood Stoves for Money or \"Bounty\"",70,2104008310,"$5,330/ton (2012$)","CO2, VOC's,CO CH4, Toxics, BC"]
["Fireplaces, Hydronic Heaters, Wood Stoves","Curtailment Program       ( \"Burn Ban\")",75,"2104008100, 2104008310, 2104008610","$8,700 (2010$)","CO2, VOC's,CO CH4, Toxics, BC"]
["Fireplaces, Hydronic Heaters, Wood Stoves","Burn Dry Seasoned Wood","n/a","2104008100, 2104008310, 2104008320, 2104008330, 2104008400, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC"]
["Fireplaces, Hydronic Heaters, Wood Stoves","No visible Emissions","n/a","2104008100, 2104008310, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC"]
["Fireplaces, Hydronic Heaters, Wood Stoves","Opacity Program","n/a","2104008100, 2104008310, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC"]
["Wood Combustion Appliances","Education Campaign","n/a","2104008100, 2104008310, 2104008610","n/a","CO2, VOC's,CO CH4, Toxics, BC"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}