{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Family Info"],"read":"whole","date_system":"1900"}

{"sheet":"Family Info","index":0,"n_rows":314,"n_cols":21,"rows_kept":314,"merged":[[0,5,0,6],[0,7,0,18]]}
[{"$nulls":5},"Opacity in Percentage",null,"Certification Level in g/bhp-hr"]
["Engine Family Name","Category","Manufacturer","Displacement","Disp Units","30-S Peak Smoke","3-S Peak Smoke","CO L/H","CO SW","NMHC L/H","NMHC SW","NOX L/H","NOX SW","PM L/H","PM SW","THC L/H","THC SW","THCE L/H","THCE SW","Useful Life"]
["8ADGK0645E10","Remanufactured","Advanced Global Environmental",645,"Cubic inches",20,29,null,2,{"$nulls":3},10.6,null,0.57,null,1.24,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES;  10 YRS/ 15750 MW-HRS/ 750000 MILES;  10 YRS/ 7500 MW-HRS/ 750000 MILES"]
["8ADGK0645EB3","Remanufactured","Advanced Global Environmental",645,"Cubic inches",21,45,1.2,1.9,null,null,9.3,12,0.52,0.48,0.9,1.4,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8ADGK0710GA1","Remanufactured","Advanced Global Environmental",710,"Cubic inches",30,48,3.3,2.2,null,null,9.2,10.6,0.58,0.47,0.9,1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES;  10 YRS/ 29250 MW-HRS/ 750000 MILES"]
["8ADGK0710T2A","Remanufactured","Advanced Global Environmental",710,"Cubic inches",20,29,0.2,0.2,null,null,5.2,7.8,0.19,0.13,0.1,0.2,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8CSXK0645E02","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",12,18,null,2.7,{"$nulls":3},12.5,null,0.5,null,1.5,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES;  10 YRS/ 16125 MW-HRS/ 750000 MILES;  10 YRS/ 7500 MW-HRS/ 750000 MILES"]
["8CSXK0645E21","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",8,12,null,1.4,{"$nulls":3},12.4,null,0.29,null,1.38,null,null,"10 YRS/ 16125 MW-HRS/ 750000 MILES"]
["8CSXK0645E2X","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",11,14,null,1.3,{"$nulls":3},14,null,0.32,null,1.28,null,null,"10 YRS/ 16125 MW-HRS/ 750000 MILES"]
["8CSXK0645E3W","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",17,35,1.7,1.7,null,null,8.1,9.3,0.39,0.39,0.94,1.13,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8CSXK0645E3X","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",21,29,1.2,1.5,null,null,8.8,10.1,0.42,0.44,0.96,1.18,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8CSXK0645E3Y","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",12,16,1,1.4,null,null,8.8,10,0.39,0.4,0.93,1.13,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8CSXK0645E3Z","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",12,14,1.1,1.3,null,null,9,11.6,0.37,0.39,0.91,1.15,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8CSXK0645EC2","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",16,27,null,1.6,{"$nulls":3},12.6,null,0.38,null,1.9,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES"]
["8CSXK0645F3Y","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",15,21,1.8,1.4,null,null,8.5,10.2,0.46,0.42,1,1.07,null,null,"10 YRS/ 23250 MW-HRS/ 750000 MILES"]
["8CSXK0710EC2","Remanufactured","CSX Transportation, Inc.",710,"Cubic inches",26,49,1.6,1.7,null,null,8.8,8.7,0.56,0.45,0.94,0.89,null,null,"10 YRS/ 30750 MW-HRS"]
["8CSXK0710ES2","Remanufactured","CSX Transportation, Inc.",710,"Cubic inches",17,22,1.1,1.5,null,null,8.7,8.9,0.33,0.34,0.86,0.99,null,null,"10 YRS/ 30750 MW-HRS"]
["8CSXK0710ES6","Remanufactured","CSX Transportation, Inc.",710,"Cubic inches",22,29,1.4,1.2,null,null,8.4,8.7,0.32,0.36,0.83,0.99,null,null,"10 YRS/ 37500 MW-HRS"]
["8CSXK0710GB0","Remanufactured","CSX Transportation, Inc.",710,"Cubic inches",30,40,2.3,1.5,null,null,8.6,10.6,0.41,0.52,0.96,1.14,null,null,"10 YRS/ 29250 MW-HRS"]
["8ECTK0645E01","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",12,18,null,2.4,{"$nulls":3},11.3,null,0.5,null,1.2,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES;  10 YRS/ 16125 MW-HRS/ 750000 MILES;  10 YRS/ 7500 MW-HRS/ 750000 MILES"]
["8ECTK0645E20","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",8,12,null,1.1,{"$nulls":3},11,null,0.3,null,1.2,null,null,"10 YRS/ 16125 MW-HRS/ 750000 MILES"]
["8ECTK0645E3A","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",17,35,1.7,1.6,null,null,8,8.6,0.4,0.4,0.9,1.1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8ECTK0645E3B","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",21,29,1.1,1.4,null,null,8.7,9.4,0.4,0.4,0.9,1.1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8ECTK0645E3C","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",12,16,0.9,1.3,null,null,8.6,9.4,0.4,0.4,0.9,1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8ECTK0645E3M","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",12,14,1.1,1.2,null,null,8.8,10.6,0.4,0.4,0.9,1.1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8ECTK0645EC1","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",16,28,null,1.5,{"$nulls":3},11.6,null,0.4,null,1.5,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES"]
["8ECTK0645F3B","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",13,16,1.9,1.5,null,null,8.5,9.3,0.4,0.4,0.9,1,null,null,"10 YRS/ 27750 MW-HRS/ 750000 MILES"]
["8ECTK0645SS1","Remanufactured","EcoTrans Environmental, Inc.",645,"Cubic inches",12,18,null,2.4,{"$nulls":3},11.3,null,0.5,null,1.2,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES"]
["8ECTK0668GE1","Remanufactured","EcoTrans Environmental, Inc.",668,"Cubic inches",18,47,2.5,2.7,null,null,9.1,10.1,0.3,0.3,0.7,0.9,null,null,"10 YRS/ 30750 MW-HRS"]
["8ECTK0710EC1","Remanufactured","EcoTrans Environmental, Inc.",710,"Cubic inches",26,49,1.6,1.7,null,null,8.8,8.7,0.6,0.5,0.9,0.9,null,null,"10 YRS/ 30750 MW-HRS"]
["8ECTK0710ES1","Remanufactured","EcoTrans Environmental, Inc.",710,"Cubic inches",17,22,1.1,1.3,null,null,8.6,8.2,0.3,0.3,0.8,0.9,null,null,"10 YRS/ 30750 MW-HRS"]
["8ECTK0710ES2","Remanufactured","EcoTrans Environmental, Inc.",710,"Cubic inches",22,29,1.4,1.1,null,null,8.3,8.1,0.3,0.4,0.8,0.9,null,null,"10 YRS/ 37500 MW-HRS"]
["8ECTK0710G3A","Remanufactured","EcoTrans Environmental, Inc.",710,"Cubic inches",24,33,3.8,2.4,null,null,8.9,12.3,0.4,0.4,0.7,0.8,null,null,"10 YRS/ 23250 MW-HRS"]
["8ECTK0710G3B","Remanufactured","EcoTrans Environmental, Inc.",710,"Cubic inches",30,40,2.2,1.5,null,null,8.4,10,0.4,0.5,1,1.1,null,null,"10 YRS/ 29250 MW-HRS"]
["8EMDG0710ES4","Fresh","Electro-Motive Diesel, Inc.",710,"Cubic inches",12,21,0.9,0.6,null,null,5.4,6.4,0.11,0.18,0.17,0.31,null,null,"10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8EMDG0710GT2","Fresh","Electro-Motive Diesel, Inc.",710,"Cubic inches",9,16,0.9,0.7,null,null,5.4,6.7,0.13,0.21,0.16,0.3,null,null,"10 YRS/ 15750 MW-HRS;  10 YRS/ 24000 MW-HRS;  10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8EMDK0645EAL","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",26,40,4.7,2.4,null,null,8.1,8.3,0.54,0.45,0.44,0.96,null,null,"10 YRS/ 750000 MILES"]
["8EMDK0645EBL","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",28,39,null,2.4,{"$nulls":3},11.2,null,0.45,null,1.09,null,null,"10 YRS/ 750000 MILES"]
["EPA - OTAQ - 5/22/09","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",11,21,1.8,1.4,null,null,15.5,16.2,0.4,0.35,0.36,0.73,null,null,"10 YRS/ 750000 MILES"]
["8EMDK0645EFT","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",28,46,2,1.5,null,null,8.1,9.8,0.56,0.47,0.36,0.63,null,null,"10 YRS/ 750000 MILES"]
["8EMDK0710EJ0","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",12,19,1.2,1.4,null,null,9.1,8.8,0.22,0.28,0.27,0.43,null,null,"10 YRS/ 24000 MW-HRS;  10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8EMDK0710ES1","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",19,29,1.3,1,null,null,9.3,10,0.21,0.26,0.28,0.44,null,null,"10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8EMDK0710ES2","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",19,30,1.5,1.7,null,null,9.1,8.7,0.24,0.29,0.2,0.34,null,null,"10 YRS/ 33750 MW-HRS;  10 YRS/ 39000 MW-HRS"]
["8EMDK0710ES3","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",20,33,1.1,0.8,null,null,6.8,7.4,0.14,0.2,0.27,0.41,null,null,"10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8EMDK0710ES4","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",12,21,0.9,0.6,null,null,5.4,6.4,0.11,0.18,0.17,0.31,null,null,"10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8EMDK0710GT2","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",20,48,1.1,1,null,null,4.9,6.6,0.14,0.22,0.2,0.38,null,null,"10 YRS/ 16500 MW-HRS/ 750000 MILES;  10 YRS/ 24000 MW-HRS/ 750000 MILES;  10 YRS/ 31500 MW-HRS/ 750000 MILES;  10 YRS/ 33750 MW-HRS/ 750000 MILES"]
["8EMDK0710MJ0","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",15,19,1.6,0.8,null,null,8.9,10.6,0.3,0.26,0.3,0.84,null,null,"10 YRS/ 28500 MW-HRS;  10 YRS/ 30000 MW-HRS"]
["8EMDK0710MJA","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",14,31,1.6,0.9,null,null,7.8,9.1,0.52,0.32,0.68,0.82,null,null,"10 YRS/ 24000 MW-HRS;  10 YRS/ 30750 MW-HRS"]
["8EMDK0710TEJ","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",8,14,0.9,0.6,null,null,7.2,9.5,0.12,0.18,0.12,0.24,null,null,"10 YRS/ 30000 MW-HRS"]
["8EMDK16.5ES2","Remanufactured","Electro-Motive Diesel, Inc.",16.5,"Liters",15,32,1.9,1.4,null,null,8,8.4,0.26,0.27,0.74,1.24,null,null,"10 YRS/ 46500 MW-HRS"]
["8GETG0958EFB","Fresh","Transportation Systems Business Operations of General Electric Company",958,"Cubic inches",9,14,0.4,0.6,null,null,5.3,5.9,0.1,0.13,0.16,0.27,null,null,"10 YRS/ 33750 MW-HRS"]
["8GETK0645MFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",19,27,3.2,3.5,null,null,9.4,12.2,0.48,0.65,0.9,1.43,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["8GETK0645MFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",20,38,2.5,2.3,null,null,8.6,10.8,0.55,0.56,0.86,1.23,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["8GETK0645MFE","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",19,31,1.8,2.2,null,null,10,12.4,0.37,0.38,0.57,0.83,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["8GETK0645MSA","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",18,20,null,4.1,{"$nulls":3},12,null,0.66,null,2.08,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["8GETK0668EFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",22,33,1.2,1.3,null,null,7.8,10.1,0.24,0.36,0.41,0.65,null,null,"10 YRS/ 30000 MW-HRS;  10 YRS/ 30750 MW-HRS"]
["8GETK0668EFB","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",26,36,1,1.3,null,null,7.8,10.4,0.26,0.41,0.41,0.65,null,null,"10 YRS/ 30750 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8GETK0668EFD","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",17,28,0.9,1.2,null,null,8.7,11.2,0.17,0.29,0.39,0.64,null,null,"10 YRS/ 30750 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["8GETK0668EFF","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",25,30,1,1.2,null,null,7,10.2,0.17,0.28,0.31,0.5,null,null,"10 YRS/ 33750 MW-HRS"]
["8GETK0668EPC","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",16,27,0.9,1.5,null,null,9,11.7,0.17,0.29,0.4,0.68,null,null,"10 YRS/ 31875 MW-HRS"]
["8GETK0668EPD","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",24,32,1.1,1.5,null,null,8.4,11.3,0.21,0.41,0.39,0.7,null,null,"10 YRS/ 24750 MW-HRS"]
["8GETK0668MFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",33,40,1.3,2.3,null,null,7.7,9.5,0.27,0.43,0.49,1.03,null,null,"10 YRS/ 30750 MW-HRS"]
["8GETK0668MFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",23,34,1.7,3,null,null,12.5,15.6,0.24,0.45,0.69,1.27,null,null,"10 YRS/ 24000 MW-HRS"]
["8GETK0710MFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",710,"Cubic inches",24,27,4.2,2.5,null,null,11.1,15.2,0.38,0.37,0.72,1.15,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["8GETK0710MFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",710,"Cubic inches",19,24,2.5,1.2,null,null,8.9,12.4,0.31,0.26,0.44,0.72,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["8GETK0958EFB","Remanufactured","Transportation Systems Business Operations of General Electric Company",958,"Cubic inches",10,15,0.9,1.7,null,null,5.5,5.4,0.13,0.15,0.3,0.41,null,null,"10 YRS/ 33750 MW-HRS"]
["8GETK0958EFF","Remanufactured","Transportation Systems Business Operations of General Electric Company",958,"Cubic inches",17,25,0.4,0.6,null,null,5.2,5.9,0.14,0.23,0.2,0.3,null,null,"10 YRS/ 33750 MW-HRS"]
["8GETK0959EFB","Remanufactured","Transportation Systems Business Operations of General Electric Company",959,"Cubic inches",32,40,1.2,1.8,null,null,7.9,8.8,0.34,0.46,0.48,0.84,null,null,"10 YRS/ 46875 MW-HRS"]
["8GETK0959EFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",959,"Cubic inches",21,25,0.4,0.8,null,null,8.8,10.9,0.14,0.18,0.41,0.65,null,null,"10 YRS/ 46875 MW-HRS"]
["8KBIK0645E3B","Remanufactured","HK Engine Components LLC",645,"Cubic inches",24,31,3.6,3.5,null,null,9.1,12.2,0.6,0.7,0.9,2,null,null,"10 YRS/ 22500 MW-HRS"]
["8KBIK0645ECZ","Remanufactured","HK Engine Components LLC",645,"Cubic inches",37,49,null,2.4,{"$nulls":3},12.6,null,0.68,null,1.26,null,null,"10 YRS/ 11250 MW-HRS;  10 YRS/ 15000 MW-HRS;  10 YRS/ 7500 MW-HRS"]
["8KBIK0710G3C","Remanufactured","HK Engine Components LLC",710,"Cubic inches",39,49,2.7,2.9,null,null,7.6,8,0.55,0.7,0.68,1.05,null,null,"10 YRS/ 30000 MW-HRS"]
["8KCSK0645E01","Remanufactured","Kansas City Southern Railroad",645,"Cubic inches",18,30,null,2.5,{"$nulls":3},11.6,null,0.62,null,1,null,null,"10 YRS/ 15750 MW-HRS/ 750000 MILES"]
["8KCSK0645E02","Remanufactured","Kansas City Southern Railroad",645,"Cubic inches",27,48,1.4,2,null,null,8.8,10.7,0.5,0.55,0.8,1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["8KCSK0710E03","Remanufactured","Kansas City Southern Railroad",710,"Cubic inches",18,27,0.9,1,null,null,8.2,9.1,0.52,0.52,0.7,0.8,null,null,"10 YRS/ 30000 MW-HRS/ 750000 MILES"]
["8MPIK0170MPD","Remanufactured","MotivePower Inc.",4.31,"Liters",28,39,null,1.8,{"$nulls":3},11.8,null,0.34,null,0.86,null,null,"10 YRS/ 6150 MW-HRS/ 750000 MILES"]
["8MPIK0645E30","Remanufactured","MotivePower Inc.",645,"Cubic inches",33,26,2.3,3.8,null,null,8.3,9.3,0.33,0.36,0.33,0.5,null,null,"10 YRS/ 24435 MW-HRS/ 750000 MILES"]
["8MPIK0645F3B","Remanufactured","MotivePower Inc.",645,"Cubic inches",36,43,1.7,2,null,null,6.8,9.7,0.4,0.46,0.47,0.71,null,null,"10 YRS/ 28688 MW-HRS"]
["8MPIK0645T2R","Remanufactured","MotivePower Inc.",645,"Cubic inches",25,41,0.3,0.3,null,null,5.2,6.3,0.19,0.18,0.15,0.13,null,null,"10 YRS/ 28688 MW-HRS/ 750000 MILES"]
["8MPIK4.31MPC","Remanufactured","MotivePower Inc.",4.31,"Liters",20,27,null,1.5,{"$nulls":3},7,null,0.15,null,0.37,null,null,"10 YRS/ 9430 MW-HRS"]
["8NREG0019LOC","Fresh","National Railway Equipment Co.",19,"Liters",12,12,0.9,1.5,null,null,2.8,3.4,0.03,0.06,0.02,0.04,null,null,"10 YRS/ 10500 MW-HRS"]
["8NREG0060LOC","Fresh","National Railway Equipment Co.",19,"Liters",12,30,0.7,1.1,null,null,2.8,2.7,0.06,0.07,0.08,0.1,null,null,"10 YRS/ 15750 MW-HRS"]
["8NREK0645ENP","Remanufactured","National Railway Equipment Co.",645,"Cubic inches",22,22,2.6,2.2,null,null,9.1,11,0.54,0.62,0.26,0.23,null,null,"10 YRS/ 17250 MW-HRS;  10 YRS/ 22500 MW-HRS;  10 YRS/ 26250 MW-HRS;  10 YRS/ 27000 MW-HRS"]
["8NREK0645ERT","Remanufactured","National Railway Equipment Co.",645,"Cubic inches",25,24,null,5.8,{"$nulls":3},6.1,null,0.45,null,0.91,null,null,"10 YRS/ 11250 MW-HRS;  10 YRS/ 15000 MW-HRS;  10 YRS/ 7500 MW-HRS"]
["8RHTK15.9BD2","Remanufactured","Railpower Hybrid Technologies Corp",1.984,"Liters",17,37,null,0.7,{"$nulls":3},3,null,0.13,null,0.22,null,null,"10 YRS/ 14490 MW-HRS;  10 YRS/ 15000 MW-HRS"]
["9ADGK0645E01","Remanufactured","Advanced Global Environmental",645,"Cubic inches",18,30,null,2.5,{"$nulls":3},11.9,null,0.63,null,1.07,null,null,"10 YRS/ 15750 MW-HRS/ 750000 MILES"]
["9ADGK0645E02","Remanufactured","Advanced Global Environmental",645,"Cubic inches",27,48,1.4,2,null,null,8.8,10.7,0.5,0.55,0.8,1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["9ADGK0668GE2","Remanufactured","Advanced Global Environmental",668,"Cubic inches",25,42,1.6,2.4,null,null,8.6,10.1,0.35,0.48,0.48,0.75,null,null,"10 YRS/ 17250 MW-HRS/ 750000 MILES;  10 YRS/ 22500 MW-HRS/ 750000 MILES;  10 YRS/ 30750 MW-HRS/ 750000 MILES"]
["9ADGK0710T2A","Remanufactured","Advanced Global Environmental",710,"Cubic inches",20,29,0.2,0.2,null,null,5.2,7.8,0.19,0.13,0.11,0.27,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES;  10 YRS/ 29250 MW-HRS/ 750000 MILES"]
["9BNRK0263LNG","Remanufactured","Burlington Northern Santa Fe Railway",263,"Cubic inches",16,22,2.6,3.3,0,"0.0",2.8,3.8,0.05,0.05,{"$nulls":4},"10 YRS/ 10125 MW-HRS/ 750000 MILES"]
["9BNRK0645E3D","Remanufactured","Burlington Northern Santa Fe Railway",645,"Cubic inches",26,44,2.3,1.9,null,null,5.1,7.4,0.49,0.46,0.97,1.22,null,null,"10 YRS/ 18750 MW-HRS/ 750000 MILES"]
["9CEXG50.0AAA","Fresh","Cummins Inc.",3.13,"Liters",40,50,0.8,1.2,null,null,3.6,3.9,0.08,0.11,0.09,0.22,null,null,"10 YRS/ 11300 MW-HRS"]
["9CEXG50.0AAB","Fresh","Cummins Inc.",3.13,"Liters",40,50,0.8,1.2,null,null,3.6,3.9,0.08,0.11,0.09,0.22,null,null,"10 YRS/ 11300 MW-HRS"]
["9CSXK0645E02","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",12,18,null,2.7,{"$nulls":3},12.5,null,0.5,null,1.5,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES;  10 YRS/ 16125 MW-HRS/ 750000 MILES;  10 YRS/ 7500 MW-HRS/ 750000 MILES"]
["9CSXK0645E21","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",8,12,null,1.4,{"$nulls":3},12.4,null,0.29,null,1.38,null,null,"10 YRS/ 16125 MW-HRS/ 750000 MILES"]
["9CSXK0645E2X","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",11,14,null,1.3,{"$nulls":3},14,null,0.32,null,1.28,null,null,"10 YRS/ 16125 MW-HRS/ 750000 MILES"]
["9CSXK0645E3X","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",21,29,1.2,1.5,null,null,8.8,10.1,0.42,0.44,0.96,1.18,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["9CSXK0645E3Y","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",12,16,1,1.4,null,null,8.8,10,0.39,0.4,0.93,1.13,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["9CSXK0645E3Z","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",12,14,1.1,1.3,null,null,9,11.6,0.37,0.39,0.91,1.15,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["9CSXK0645EC2","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",16,27,null,1.6,{"$nulls":3},12.6,null,0.38,null,1.9,null,null,"10 YRS/ 11250 MW-HRS/ 750000 MILES"]
["9CSXK0645F3Y","Remanufactured","CSX Transportation, Inc.",645,"Cubic inches",15,21,1.8,1.4,null,null,8.5,10.2,0.46,0.42,1,1.07,null,null,"10 YRS/ 23250 MW-HRS/ 750000 MILES"]
["9EMDG0710ES4","Fresh","Electro-Motive Diesel, Inc.",710,"Cubic inches",12,21,0.8,0.5,null,null,5.4,6.4,0.13,0.17,0.13,0.21,null,null,"10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["9EMDG0710GT2","Fresh","Electro-Motive Diesel, Inc.",710,"Cubic inches",9,16,0.9,0.6,null,null,5.4,6.7,0.15,0.2,0.12,0.2,null,null,"10 YRS/ 15750 MW-HRS;  10 YRS/ 24000 MW-HRS;  10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["9EMDK0645EAL","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",26,40,3.6,2.2,null,null,8.1,8.3,0.45,0.41,0.35,0.68,null,null,"10 YRS/ 750000 MILES"]
["9EMDK0645EBL","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",28,39,null,2.4,{"$nulls":3},11.2,null,0.45,null,1.09,null,null,"10 YRS/ 750000 MILES"]
["9EMDK0645EFC","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",11,21,0.7,1.5,null,null,15.5,16.2,0.32,0.31,0.27,0.45,null,null,"10 YRS/ 750000 MILES"]
["9EMDK0645EFT","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",28,46,1,1.6,null,null,8.1,9.8,0.48,0.43,0.28,0.36,null,null,"10 YRS/ 750000 MILES"]
["9EMDK0645RBL","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",14,25,null,1.5,{"$nulls":3},11,null,0.21,null,0.76,null,null,"10 YRS/ 750000 MILES"]
["9EMDK0645TEF","Remanufactured","Electro-Motive Diesel, Inc.",645,"Cubic inches",14,24,1.2,1.4,null,null,7.2,9.3,0.14,0.18,0.18,0.49,null,null,"10 YRS/ 750000 MILES"]
["9EMDK0710EJ0","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",12,19,1.2,1.4,null,null,9.1,8.8,0.24,0.26,0.23,0.33,null,null,"10 YRS/ 24000 MW-HRS;  10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["9EMDK0710ES1","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",19,29,1.2,0.9,null,null,9.3,10,0.22,0.24,0.24,0.34,null,null,"10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["9EMDK0710ES2","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",19,30,1.4,1.7,null,null,9.1,8.7,0.25,0.28,0.16,0.23,null,null,"10 YRS/ 33750 MW-HRS;  10 YRS/ 39000 MW-HRS"]
["9EMDK0710ES3","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",20,33,1,0.7,null,null,6.8,7.4,0.16,0.19,0.23,0.31,null,null,"10 YRS/ 31500 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["9EMDK0710GT2","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",20,48,1,1,null,null,4.9,6.6,0.16,0.21,0.16,0.27,null,null,"10 YRS/ 16500 MW-HRS/ 750000 MILES;  10 YRS/ 24000 MW-HRS/ 750000 MILES;  10 YRS/ 31500 MW-HRS/ 750000 MILES;  10 YRS/ 33750 MW-HRS/ 750000 MILES"]
["9EMDK0710MJ0","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",15,19,0.5,0.8,null,null,8.9,10.6,0.22,0.23,0.22,0.57,null,null,"10 YRS/ 30750 MW-HRS;  10 YRS/ 31500 MW-HRS"]
["9EMDK0710MJA","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",14,31,0.5,0.9,null,null,7.8,9.1,0.44,0.28,0.59,0.55,null,null,"10 YRS/ 24000 MW-HRS;  10 YRS/ 30750 MW-HRS"]
["9EMDK0710TEJ","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",8,14,0.9,0.6,null,null,7.2,9.5,0.12,0.18,0.12,0.24,null,null,"10 YRS/ 30000 MW-HRS"]
["9EMDK0710TMA","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",26,40,1.5,0.9,null,null,7.7,10,0.16,0.18,0.14,0.25,null,null,"10 YRS/ 22500 MW-HRS;  10 YRS/ 28500 MW-HRS"]
["9EMDK0710TMJ","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",16,28,1.2,0.7,null,null,7.3,10,0.16,0.19,0.15,0.29,null,null,"10 YRS/ 30000 MW-HRS"]
["9EMDK0710TS1","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",21,41,1.6,0.8,null,null,7.2,9.6,0.17,0.18,0.15,0.25,null,null,"10 YRS/ 30000 MW-HRS;  10 YRS/ 32550 MW-HRS"]
["9EMDK0710TS3","Remanufactured","Electro-Motive Diesel, Inc.",710,"Cubic inches",15,21,0.9,0.7,null,null,6.9,8,0.14,0.18,0.14,0.24,null,null,"10 YRS/ 30000 MW-HRS;  10 YRS/ 32250 MW-HRS"]
["9EMDK16.5ES2","Remanufactured","Electro-Motive Diesel, Inc.",16.5,"Liters",15,32,1.9,1.4,null,null,8,8.4,0.26,0.27,0.74,1.24,null,null,"10 YRS/ 46500 MW-HRS"]
["9GETG0958EFB","Fresh","Transportation Systems Business Operations of General Electric Company",958,"Cubic inches",16,26,0.4,0.4,null,null,4.9,5.3,0.11,0.11,0.15,0.21,null,null,"10 YRS/ 33750 MW-HRS"]
["9GETK0645MFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",19,27,3.2,3.5,null,null,9.4,12.2,0.48,0.65,0.9,1.43,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["9GETK0645MFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",20,38,2.5,2.3,null,null,8.6,10.8,0.55,0.56,0.86,1.23,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["9GETK0645MFE","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",19,31,1.8,2.2,null,null,10,12.4,0.37,0.38,0.57,0.83,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["9GETK0645MSA","Remanufactured","Transportation Systems Business Operations of General Electric Company",645,"Cubic inches",18,20,null,4.1,{"$nulls":3},12,null,0.66,null,2.08,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["9GETK0668EFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",22,33,1.2,1.3,null,null,7.8,10.1,0.24,0.36,0.41,0.65,null,null,"10 YRS/ 30000 MW-HRS;  10 YRS/ 30750 MW-HRS"]
["9GETK0668EFB","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",26,36,1,1.3,null,null,7.8,10.4,0.26,0.41,0.41,0.65,null,null,"10 YRS/ 30750 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["9GETK0668EFD","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",17,28,0.9,1.2,null,null,8.7,11.2,0.17,0.29,0.39,0.64,null,null,"10 YRS/ 30750 MW-HRS;  10 YRS/ 33750 MW-HRS"]
["9GETK0668EFF","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",25,30,1,1.2,null,null,7,10.2,0.17,0.28,0.31,0.5,null,null,"10 YRS/ 33750 MW-HRS"]
["9GETK0668EPC","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",16,27,0.9,1.5,null,null,9,11.7,0.17,0.29,0.4,0.68,null,null,"10 YRS/ 31875 MW-HRS"]
["9GETK0668EPD","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",24,32,1.1,1.5,null,null,8.4,11.3,0.21,0.41,0.39,0.7,null,null,"10 YRS/ 24750 MW-HRS"]
["9GETK0668MFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",33,40,1.3,2.3,null,null,7.7,9.5,0.27,0.43,0.49,1.03,null,null,"10 YRS/ 30750 MW-HRS"]
["9GETK0668MFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",668,"Cubic inches",23,34,1.7,3,null,null,12.5,15.6,0.24,0.45,0.69,1.27,null,null,"10 YRS/ 24000 MW-HRS"]
["9GETK0710MFA","Remanufactured","Transportation Systems Business Operations of General Electric Company",710,"Cubic inches",24,27,4.2,2.5,null,null,11.1,15.2,0.38,0.37,0.72,1.15,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["9GETK0710MFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",710,"Cubic inches",19,24,2.5,1.2,null,null,8.9,12.4,0.31,0.26,0.44,0.72,null,null,"10 YRS/ 750000 MW-HRS/ 750000 MILES"]
["9GETK0958EFB","Remanufactured","Transportation Systems Business Operations of General Electric Company",958,"Cubic inches",10,15,0.9,1.7,null,null,5.5,5.4,0.13,0.15,0.3,0.41,null,null,"10 YRS/ 33750 MW-HRS"]
["9GETK0958EFF","Remanufactured","Transportation Systems Business Operations of General Electric Company",958,"Cubic inches",17,25,0.4,0.6,null,null,5.2,5.9,0.14,0.23,0.2,0.3,null,null,"10 YRS/ 33750 MW-HRS"]
["9GETK0959EFB","Remanufactured","Transportation Systems Business Operations of General Electric Company",959,"Cubic inches",32,40,1.2,1.8,null,null,7.9,8.8,0.34,0.46,0.48,0.84,null,null,"10 YRS/ 46875 MW-HRS"]
["9GETK0959EFC","Remanufactured","Transportation Systems Business Operations of General Electric Company",959,"Cubic inches",21,25,0.4,0.8,null,null,8.8,10.9,0.14,0.18,0.41,0.65,null,null,"10 YRS/ 46875 MW-HRS"]
["9KBIK0645E3B","Remanufactured","HK Engine Components LLC",645,"Cubic inches",25,46,3,3,null,null,9.3,12.2,0.45,0.45,0.9,1.28,null,null,"10 YRS/ 16875 MW-HRS;  10 YRS/ 22500 MW-HRS"]
["9KBIK0645ECZ","Remanufactured","HK Engine Components LLC",645,"Cubic inches",37,49,null,2.4,{"$nulls":3},12.6,null,0.68,null,1.26,null,null,"10 YRS/ 11250 MW-HRS;  10 YRS/ 15000 MW-HRS;  10 YRS/ 7500 MW-HRS"]
["9KBIK0710G3B","Remanufactured","HK Engine Components LLC",710,"Cubic inches",31,46,1.3,2.4,null,null,7.4,8.7,0.51,0.66,0.58,0.86,null,null,"10 YRS/ 30000 MW-HRS"]
["9KBIK0710G3C","Remanufactured","HK Engine Components LLC",710,"Cubic inches",39,49,2.7,2.9,null,null,7.6,8,0.55,0.7,0.68,1.05,null,null,"10 YRS/ 30000 MW-HRS"]
["9KCSK0645E01","Remanufactured","Kansas City Southern Railroad",645,"Cubic inches",18,30,null,2.5,{"$nulls":3},11.6,null,0.62,null,1,null,null,"10 YRS/ 15750 MW-HRS/ 750000 MILES"]
["9KCSK0645E02","Remanufactured","Kansas City Southern Railroad",645,"Cubic inches",27,48,1.4,2,null,null,8.8,10.7,0.5,0.55,0.8,1,null,null,"10 YRS/ 22500 MW-HRS/ 750000 MILES"]
["9KCSK0645E04","Remanufactured","Kansas City Southern Railroad",645,"Cubic inches",26,33,1.5,1.4,null,null,8.2,10.8,0.5,0.55,0.6,0.8,null,null,"10 YRS/ 27000 MW-HRS/ 750000 MILES"]
["9MPIK0170MPD","Remanufactured","MotivePower Inc.",4.31,"Liters",28,39,null,1.8,{"$nulls":3},11.8,null,0.34,null,0.86,null,null,"10 YRS/ 6150 MW-HRS/ 750000 MILES"]
["9MPIK0645F3B","Remanufactured","MotivePower Inc.",645,"Cubic inches",36,43,1.7,2,null,null,6.8,9.7,0.4,0.46,0.47,0.71,null,null,"10 YRS/ 28688 MW-HRS"]
["9MPIK0645M2R","Remanufactured","MotivePower Inc.",645,"Cubic inches",26,41,0.3,0.3,null,null,5.2,6.3,0.14,0.14,0.15,0.13,null,null,"10 YRS/ 28688 MW-HRS/ 750000 MILES"]
["9NREG0019LOC","Fresh","National Railway Equipment Co.",3.17,"Liters",12,12,1.1,1.8,null,null,2.7,2.4,0.08,0.09,0.08,0.13,null,null,"10 YRS/ 10500 MW-HRS"]
["9NREG0060LOC","Fresh","National Railway Equipment Co.",3.17,"Liters",12,30,0.1,1.4,null,null,2.8,2.5,0.06,0.09,0.06,0.08,null,null,"10 YRS/ 15750 MW-HRS"]
["9NREK0645ENP","Remanufactured","National Railway Equipment Co.",645,"Cubic inches",22,22,2.6,2.2,null,null,9.1,11,0.54,0.62,0.26,0.23,null,null,"10 YRS/ 17250 MW-HRS;  10 YRS/ 22500 MW-HRS;  10 YRS/ 26250 MW-HRS;  10 YRS/ 27000 MW-HRS"]
["9NREK0645ERT","Remanufactured","National Railway Equipment Co.",645,"Cubic inches",25,24,null,5.8,{"$nulls":3},6.1,null,0.45,null,0.91,null,null,"10 YRS/ 11250 MW-HRS;  10 YRS/ 15000 MW-HRS;  10 YRS/ 7500 MW-HRS"]
["9OCNK0645ERB","Remanufactured","OceanAir Environmental, LLC",10.6,"Liters",10,15,0,1.3,null,null,0,6.1,0,0.2,0,0.56,null,null,"11200 MW-HRS/ 750000 MILES;  11250 MW-HRS/ 750000 MILES;  15000 MW-HRS/ 750000 MILES;  7500 MW-HRS/ 750000 MILES"]
["6CSXK0645E21","Reman","CSXT Environmental Corporation",645,"cubic inches",7.5,12,0,1.4,"no data","no data",0,12.4,0,0.29,0,1.38,"no data","no data",null,{"v":750000,"d":"750,000"}]
["6CSXK0645EC2","Reman","CSXT Environmental Corporation",645,"cubic inches",16.4,27.8,0,1.6,"no data","no data",0,12.6,0,0.38,0,1.89,"no data","no data",null,{"v":750000,"d":"750,000"}]
["6CSXK0645E02","Reman","CSXT Environmental Corporation",645,"cubic inches",11.5,18,0,2.7,"no data","no data",0,12.5,0,0.49,0,1.46,"no data","no data",null,{"v":750000,"d":"750,000"}]
["6ECTK0668GE1","Reman","EcoTrans Environmental, Inc",668,"cubic inches",18,47,2.5,2.7,"no data","no data",9.1,10.1,0.31,0.34,0.74,0.86,"no data","no data",{"v":30750,"d":"30,750"}]
["6RHTK0121BD1","Reman","RailPower Hybrid Technologies, Corp.",121,"cubic inches",18.8,24.8,null,1.1,"no data","no data","no data",5,"no data",0.15,"no data",0.27,"no data","no data",{"v":15750,"d":"15,750"}]
["6NREK0645ERT","Reman","National Railway Equipment Company",645,"cubic inches",24.7,24.3,null,5.8,"no data",0,"no data",6.1,"no data",0.45,"no data",0.91,"no data","no data",null,{"v":750000,"d":"750,000"}]
["7NREG0060LOC","F","NAT RAILWAY",3.13,"LITERS",12,30,0.8,1.2,"no data","no data",2.8,2.7,0.06,0.07,0.08,0.1,"no data","no data","10YRS"]
["7MPIK0645E30","R","MOTIVE POWER",645,"CI",33,26,2.3,3.8,"no data","no data",8.3,9.3,0.33,0.36,0.33,0.5,"no data","no data","10YRS/22500MW"]
["7MPIK0170MPD","R","MOTIVE POWER",4.31,"LITERS",28,39,null,1.8,"no data","no data","no data",11.8,"no data",0.34,"no data",0.86,"no data","no data","10YRS/6150MW"]
["7RHTK15.9BD2","R","RAILPOWER",1.984,"LITERS",17,37,0.4,0.7,"no data","no data",3.3,2.9,0.13,0.13,0.1,0.22,"no data","no data","10YRS/15000MW"]
["7GETK0710MFA","R","GE",710,"CI",24,27,4.2,2.5,"no data","no data",11.1,15.2,0.38,0.37,0.72,1.15,"no data","no data","10YRS"]
["7GETK0645MFA","R","GE",645,"CI",19,27,3.2,3.5,"no data","no data",9.4,12.2,0.48,0.65,0.9,1.43,"no data","no data","10YRS"]
["7GETK0668MFA","R","GE",668,"CI",33,40,1.3,2.3,"no data","no data",7.7,9.5,0.27,0.43,0.49,1.03,"no data","no data","10 YRS"]
["7GETK0958EFB","R","GE",958,"CI",10,15,0.9,1.7,"no data","no data",5.5,5.4,0.13,0.15,0.3,0.41,"no data","no data","10YRS"]
["7GETK0645MFC","R","GE",645,"CI",20,38,2.5,2.3,"no data","no data",8.6,10.8,0.55,0.56,0.86,1.23,"no data","no data","10TRS"]
["7GETK0645MSA","R","GE",645,"CI",18,20,null,4.1,"no data","no data","no data",12,"no data",0.66,"no data",2.08,"no data","no data","10YRS"]
["7GETK0710MFC","R","GE",710,"CI",19,24,2.5,1.2,"no data","no data",8.9,12.4,0.31,0.26,0.44,0.72,"no data","no data","10YRS"]
["7MPIK0645F3B","R","MOTIVE POWER",645,"CI",36,43,1.7,2,"no data","no data",6.8,9.7,0.4,0.46,0.47,0.71,"no data","no data","10YRS"]
["7GETK0710MFE","R","GE",710,"CI",16,20,2.7,1.2,"no data","no data",10.2,14.5,0.31,0.25,0.45,0.76,"no data","no data","10YRS"]
["7GETK0959EFB","R","GE",959,"CI",32,40,1.2,1.8,"no data","no data",7.9,8.8,0.34,0.46,0.48,0.84,"no data","no data","10YRS"]
["7GETK0645MFE","R","GE",645,"CI",19,31,1.8,2.2,"no data","no data",10,12.4,0.37,0.38,0.57,0.83,"no data","no data","10YRS"]
["7GETK0959EFC","R","GE",959,"CI",31,40,1,1.5,"no data","no data",9.3,11.4,0.28,0.41,0.51,0.81,"no data","no data","10YRS"]
["7GETK0668EPC","R","GE",668,"CI",30,41,0.9,1.5,"no data","no data",9,11.7,0.17,0.29,0.4,0.68,"no data","no data","10YRS"]
["7NREG0019LOC","F","NAT RAILWAY",3.16,"LITERS",9,9,0.9,1.5,"no data","no data",2.8,3.4,0.03,0.06,0.02,0.04,"no data","no data","10YRS"]
["7NREK0645ENP","R","NAT RAILWAY",645,"CI",22,22,2.6,2.2,"no data","no data",9.1,11,0.54,0.62,0.26,0.23,"no data","no data","10YRS"]
["7GETK0668EFA","R","GE",668,"CI",22,33,1.2,1.3,"no data","no data",7.8,10.1,0.24,0.36,0.41,0.65,"no data","no data","10YRS"]
["7GETK0668EFD","R","GE",668,"CI",17,28,0.9,1.2,"no data","no data",8.7,11.2,0.17,0.29,0.39,0.64,"no data","no data","10YRS"]
["7GETK0668EFF","R","GE",668,"CI",20,24,0.8,1,"no data","no data",7,10.2,0.09,0.13,0.24,0.38,"no data","no data","10YRS"]
["7GETK0668EFB","R","GE",668,"CI",26,36,1,1.3,"no data","no data",7.8,10.4,0.26,0.41,0.41,0.65,"no data","no data","10YRS"]
["7GETK0958EFF","R","GE",958,"CI",17,25,0.4,0.6,"no data","no data",5.2,5.9,0.14,0.23,0.2,0.3,"no data","no data","10YRS"]
["7GETG0958EFB","F","GE",958,"CI",10,15,0.9,1.7,"no data","no data",5.5,5.4,0.13,0.15,0.3,0.41,"no data","no data","10YRS"]
["7NREK0645ERT","R","NAT RAILWAY",645,"CI",25,24,6,5.8,"no data","no data",6,6.1,0.63,0.45,0.64,0.91,"no data","no data","10YRS"]
["7CSXK0710ES6","R","CSX",710,"CI",22,29,1.4,1.2,"no data","no data",8.4,8.7,0.32,0.36,0.83,0.99,"no data","no data","10 YRS/ 37500MW-HRS"]
["7CSXK0710ES2","R","CSX",710,"CI",17,22,1.1,1.5,"no data","no data",8.7,8.9,0.33,0.34,0.86,0.99,"no data","no data","10YRS/30750 MW-HRS"]
["7CSXK0710EC2","R","CSX",710,"CI",26,49,1.6,1.7,"no data","no data",8.8,8.7,0.56,0.45,0.94,0.89,"no data","no data","10 YRS/30750 MW-HRS"]
["7CSXK0710GB0","R","CSX",710,"CI",30,40,2.3,1.5,"no data","no data",8.6,10.6,0.41,0.52,0.96,1.14,"no data","no data","10 YRS/29250 MW-HRS"]
["7CSXK0645E3Z","R","CSX",645,"CI",12,14,1.1,1.3,"no data","no data",9,11.6,0.37,0.39,0.91,1.15,"no data","no data","10 YRS/750000 MI."]
["7CSXK0645E3Y","R","CSX",645,"CI",12,16,1,1.4,"no data","no data",8.8,10,0.39,0.4,0.93,1.13,"no data","no data","10 YRS/ 750000"]
["7CSXK0645E3X","R","CSX",645,"CI",21,29,1.2,1.5,"no data","no data",8.8,10.1,0.42,0.44,0.96,1.18,"no data","no data","10 YRS/ 750000"]
["7CSXK0645E3W","R","CSX",645,"CI",17,35,1.7,1.7,"no data","no data",8.1,9.3,0.39,0.39,0.94,1.13,"no data","no data","10 YRS/ 750000"]
["7CSXK0645E21","R","CSX",645,"CI",8,12,"-",12.4,"no data","no data","no data",12.4,"no data",0.29,"no data",1.38,"no data","no data","10 YRS/ 750000"]
["7CSXK0645EC2","R","CSX",645,"CI",16,27,"-",1.6,"no data","no data","no data",12.6,"no data",0.38,"no data",1.9,"no data","no data","10 YRS/ 750000"]
["7CSXK0645F02","R","CSX",645,"CI",12,18,"-",2.7,"no data","no data","no data",12.5,"no data",0.5,"no data",1.5,"no data","no data","10 YRS/ 750000"]
["7ECTK0645SS1","R","ECOTRANS",645,"CI",12,18,"-",2.4,"no data","no data","no data",11.3,"no data",0.5,"no data",1.2,"no data","no data","10 YRS/ 750000"]
["7ECTK0645F3B","R","ECOTRANS",645,"CI",13,16,1.9,1.5,"no data","no data",8.5,9.3,0.4,0.4,0.9,1,"no data","no data","10 YRS/ 750000"]
["7ECTK0645EC1","R","ECOTRANS",645,"CI",16,28,"-",1.5,"no data","no data","no data",11.6,"no data",0.4,"no data",1.5,"no data","no data","10 YRS/ 750000"]
["7ECTK0645E20","R","ECOTRANS",645,"CI",8,12,"-",1.1,"no data","no data","no data",11,"no data",0.3,"no data",1.2,"no data","no data","10 YRS/ 750000"]
["7ECTK0645E3M","R","ECOTRANS",645,"CI",12,14,1.1,1.2,"no data","no data",8.8,10.6,0.4,0.4,0.9,1.1,"no data","no data","10 YRS/ 750000"]
["7ECTK0645E3C","R","ECOTRANS",645,"CI",12,16,0.9,1.3,"no data","no data",8.6,9.4,0.4,0.4,0.9,1,"no data","no data","10 YRS/ 750000"]
["7ECTK0645E3B","R","ECOTRANS",645,"CI",21,29,1.1,1.4,"no data","no data",8.7,9.4,0.4,0.4,0.9,1.1,"no data","no data","10 YRS/ 750000"]
["7ECTK0645E3A","R","ECOTRANS",645,"CI",17,35,1.7,1.6,"no data","no data",8,8.6,0.4,0.4,0.9,1.1,"no data","no data","10 YRS/ 750000"]
["7ECTK0645E01","R","ECOTRANS",645,"CI",12,18,"-",2.4,"no data","no data","no data",11.3,"no data",0.5,"no data",1.2,"no data","no data","10 YRS/ 750000"]
["7ECTK0710G3B","R","ECOTRANS",710,"CI",30,40,2.2,1.5,"no data","no data",8.4,10,0.4,0.5,1,1.1,"no data","no data","10 YRS/ 29250 MW-HRS"]
["7ECTK0710ES2","R","ECOTRANS",710,"CI",22,29,1.4,1.1,"no data","no data",8.3,8.1,0.3,0.4,0.8,0.9,"no data","no data","10 YRS/ 37500 MW-HRS"]
["7ECTK0710ES1","R","ECOTRANS",710,"CI",17,22,1.1,1.3,"no data","no data",8.6,8.2,0.3,0.3,0.8,0.9,"no data","no data","10 YRS/ 30750 MW-HRS"]
["7EMDG0710GT2","F","EMD",710,"CI",9,16,0.9,0.7,"no data","no data",5.4,6.7,0.13,0.21,0.16,0.3,"no data","no data","32250 MW-HRS/10YRS    30000 MW-HRS/10YRS     22500 MW-HRS/10YRS     15000 MW-HRS/10YRS"]
["7EMDK16.5ES2","R","EMD",16.5,"LITERS",15,32,1.9,1.4,"no data","no data",8,8.4,0.26,0.27,0.74,1.24,"no data","no data","45000 MW-HRS/10 YRS"]
["7EMDK0645EAL","R","EMD",645,"CI",26,40,4.7,2.4,"no data","no data",8.1,8.3,0.54,0.45,0.44,0.96,"no data","no data","750000 MI/10 YRS"]
["7EMDK0645EBL","R","EMD",645,"CI",28,39,6.5,2.4,"no data","no data",10.7,11.2,0.56,0.45,0.61,1.09,"no data","no data","750000 MI/10 YRS"]
["7EMDK0645EFT","R","EMD",645,"CI",28,45,2,1.5,"no data","no data",8.1,9.8,0.56,0.47,0.36,0.63,"no data","no data","750000 MI/10 YRS"]
["7EMDK0710EJO","R","EMD",710,"CI",22,32,1.5,1.3,"no data","no data",8.6,8.7,0.29,0.33,0.43,0.61,"no data","no data","30000 MW-HRS/10 YRS     32250 MW-HRS/10 YRS"]
["7EMDK0710ES1","R","EMD",710,"CI",33,47,1.8,1.4,"no data","no data",9.2,9.8,0.33,0.36,0.5,0.77,"no data","no data","30000 MW-HRS/10 YRS       "]
["7EMDK0710ES2","R","EMD",710,"CI",19,30,1.5,1.7,"no data","no data",9.1,8.7,0.24,0.29,0.2,0.34,"no data","no data","32250 MW-HRS/10 YRS     37500 MW-HRS/10 YRS"]
["7EMDK0710ES3","R","EMD",710,"CI",20,33,1.1,0.8,"no data","no data",6.8,7.4,0.14,0.2,0.27,0.41,"no data","no data","30000 MW-HRS/10 YRS     32250 MW-HRS/10 YRS"]
["7EMDK0710MJA","R","EMD",710,"CI",14,31,1.6,0.9,"no data","no data",7.8,9.1,0.52,0.32,0.68,0.82,"no data","no data","22500 MW-HRS/10 HRS     28500 MW-HRS/10 YRS"]
["7EMDK0710MJO","R","EMD",710,"CI",15,19,1.6,0.8,"no data","no data",8.9,10.6,0.3,0.26,0.5,0.84,"no data","no data","28500 MW-HRS/10 YRS     30000 MW-HRS/10 YRS"]
["7EMDG0710ES1","R","EMD",710,"CI",12,26,0.9,0.6,"no data","no data",5,6.4,0.11,0.18,0.17,0.31,"no data","no data","32250 MW-HRS/10 YRS     30000 MW-HRS/10 YRS"]
["7EMDK0710ES4","R","EMD",710,"CI",12,21,0.9,0.6,"no data","no data",5.4,6.4,0.11,0.18,0.17,0.31,"no data","no data"]
["5NREK0645ENP","Reman","National Railway Equipment Co.",645,"cubic inches",22.1,22.2,2.6,2.2,0,0,9.1,11,0.54,0.62,0.26,0.23,0,0,null,{"v":750000,"d":"750,000"}]
["5GETg0958efb","Fresh","Transportation Systems Business Operations of General Electric Company",958,"cubic inches",9.2,14.2,0.4,0.6,0.16,0.27,5.3,5.9,0.1,0.13,0.16,0.27,0.16,0.27,{"v":33750,"d":"33,750"}]
["5ECTK0645EC1","Reman","EcoTrans Environmental, Inc",645,"cubic inches",16.4,27.8,0,1.5,null,null,0,11.6,0,0.37,0,1.53,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5ECTK0645E3A","Reman","EcoTrans Environmental, Inc",645,"cubic inches",16.5,35,1.7,1.6,null,null,8,8.6,0.39,0.37,0.92,1.05,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5ECTK0645E3B","Reman","EcoTrans Environmental, Inc",645,"cubic inches",20.5,29,1.1,1.4,null,null,8.7,9.4,0.42,0.42,0.94,1.1,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5eCtK0645E3C","Reman","EcoTrans Environmental, Inc",645,"cubic inches",11.5,16,0.9,1.3,null,null,8.6,9.4,0.39,0.39,0.91,1.05,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5ECTK0645E3M","Reman","EcoTrans Environmental, Inc",645,"cubic inches",11.5,14,1.1,1.2,null,null,8.8,10.6,0.37,0.37,0.89,1.05,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5ECTK0645F3B","Reman","EcoTrans Environmental, Inc",645,"cubic inches",12.5,16,1.9,1.5,null,null,8.5,9.3,0.41,0.39,0.88,1,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5ECTK0710G3A","Reman","EcoTrans Environmental, Inc",710,"cubic inches",23.6,32.5,3.8,2.4,null,null,8.9,12.3,0.42,0.41,0.68,0.78,null,null,{"v":23250,"d":"23,250"}]
["5ECTK0710G3B","Reman","EcoTrans Environmental, Inc",710,"cubic inches",29.5,40,2.2,1.5,null,null,8.4,10,0.41,0.51,0.95,1.09,null,null,{"v":29250,"d":"29,250"}]
["5ECTK0710EC1","Reman","EcoTrans Environmental, Inc",710,"cubic inches",25.5,48.5,1.6,1.7,null,null,8.8,8.7,0.56,0.45,0.94,0.89,null,null,{"v":30750,"d":"30,750"}]
["5ECTK0710ES1","Reman","EcoTrans Environmental, Inc",710,"cubic inches",16.7,21.9,1.1,1.3,null,null,8.6,8.2,0.33,0.33,0.84,0.92,null,null,{"v":30750,"d":"30,750"}]
["5GMXG0710ES1","Fresh","General Motors Electro-Motive Division",710,"cubic inches",12.165,26.59,1,0.6,null,null,5.1,6.6,0.07,0.18,0.22,0.39,null,null,{"v":32250,"d":"32,250"}]
["5ECTK0710ES2","Reman","EcoTrans Environmental, Inc",710,"cubic inches",21.7,28.9,1.4,1.1,null,null,8.3,8.1,0.31,0.35,0.82,0.93,null,null,{"v":37500,"d":"37,500"}]
["5ECTK0645E01","Reman","EcoTrans Environmental, Inc",645,"cubic inches",11.5,18,0,2.4,null,null,0,11.3,0,0.46,0,1.21,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5GMXK0645EBL","Reman","General Motors Electro-Motive Division",645,"cubic inches",28.335,38.85,4.5,2.3,null,null,10.9,11.6,0.47,0.41,0.41,0.84,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5GMXK0710EJ0","Reman","General Motors Electro-Motive Division",710,"cubic inches",22.205,32.06,1.5,1.3,null,null,8.6,8.7,0.29,0.33,0.43,0.61,null,null,{"v":30000,"d":"30,000"}]
["5GMXK16.5ES2","Reman","General Motors Electro-Motive Division",16.55,"liters",14.845,31.66,1.9,1.4,null,null,8,8.4,0.26,0.27,0.74,1.24,null,null,{"v":45000,"d":"45,000"}]
["5GMXK0710MJA","Reman","General Motors Electro-Motive Division",710,"cubic inches",13.855,30.83,1.6,0.9,null,null,7.8,9.1,0.52,0.32,0.68,0.82,null,null,{"v":22500,"d":"22,500"}]
["5GMXK0710MJ0","Reman","General Motors Electro-Motive Division",710,"cubic inches",14.545,18.98,1.6,0.8,null,null,8.9,10.6,0.3,0.26,0.5,0.84,null,null,{"v":28500,"d":"28,500"}]
["5GMXK0710ES2","Reman","General Motors Electro-Motive Division",710,"cubic inches",15.155,19.23,1.6,1.3,null,null,8.5,8.5,0.22,0.28,0.38,0.61,null,null,{"v":32250,"d":"32,250"}]
["5GMXK0710ES1","Reman","General Motors Electro-Motive Division",710,"cubic inches",32.545,46.99,1.8,1.4,null,null,9.2,9.8,0.33,0.36,0.5,0.77,null,null,{"v":30000,"d":"30,000"}]
["5GMXK0645ESW","Reman","General Motors Electro-Motive Division",645,"cubic inches",16.245,30.06,4.5,2.3,null,null,10.9,11.6,0.47,0.41,0.41,0.84,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5GMXK0645EFT","Reman","General Motors Electro-Motive Division",645,"cubic inches",28.475,45.41,2,1.5,null,null,8.1,9.8,0.56,0.47,0.36,0.63,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5GMXK0645EAL","Reman","General Motors Electro-Motive Division",645,"cubic inches",25.995,40.36,4.7,2.4,null,null,8.1,8.3,0.54,0.45,0.44,0.96,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5getk0645msa","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",26.1,32,null,4.1,null,2.08,null,12.3,null,0.66,null,2.08,null,2.08,null,{"v":750000,"d":"750,000"}]
["5getk0645mfa","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",23,34,3.2,3.5,0.9,1.43,10,12.5,0.48,0.65,0.9,1.43,0.9,1.43,null,{"v":750000,"d":"750,000"}]
["5getk0959efb","Reman","Transportation Systems Business Operations of General Electric Company",959,"cubic inches",32,40,1.2,1.8,0.48,0.84,7.9,8.8,0.34,0.46,0.48,0.84,0.48,0.84,{"v":46875,"d":"46,875"}]
["5getk0645mfc","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",22.2,38.2,2.5,2.3,0.86,1.23,9.1,11.3,0.55,0.56,0.86,1.23,0.86,1.23,null,{"v":750000,"d":"750,000"}]
["5getk0710mfa","Reman","Transportation Systems Business Operations of General Electric Company",710,"cubic inches",23.7,26.6,4.2,2.5,0.72,1.15,11.1,15.2,0.38,0.37,0.72,1.15,0.72,1.15,null,{"v":750000,"d":"750,000"}]
["5getk0710mfE","Reman","Transportation Systems Business Operations of General Electric Company",710,"cubic inches",16.3,20,2.7,1.2,0.45,0.76,10.2,14.5,0.31,0.25,0.45,0.76,0.45,0.76,null,{"v":750000,"d":"750,000"}]
["5getk0710mfC","Reman","Transportation Systems Business Operations of General Electric Company",710,"cubic inches",19.2,23.5,2.5,1.2,0.44,0.72,8.9,12.4,0.31,0.26,0.44,0.72,0.44,0.72,null,{"v":750000,"d":"750,000"}]
["5getk0668efd","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",31.5,44.3,0.9,1.2,0.39,0.64,8.7,11.2,0.17,0.29,0.39,0.64,0.39,0.64,{"v":33750,"d":"33,750"}]
["5getk0668eff","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",33.8,47.1,1,1.2,0.31,0.5,7,10.2,0.17,0.28,0.31,0.5,0.31,0.5,{"v":33750,"d":"33,750"}]
["5getk0668efa","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",35.6,46.9,1.7,2.4,0.55,0.77,9,11.6,0.42,0.49,0.55,0.77,0.55,0.77,{"v":30750,"d":"30,750"}]
["5getk0668efb","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",40,49.9,1,1.3,0.41,0.65,7.8,10.4,0.26,0.41,0.41,0.65,0.41,0.65,{"v":33750,"d":"33,750"}]
["5getk0645mfe","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",20.9,30.7,1.8,2.2,0.57,0.83,10.5,12.9,0.37,0.38,0.57,0.83,0.57,0.83,null,{"v":750000,"d":"750,000"}]
["5GETk0958efb","Reman","Transportation Systems Business Operations of General Electric Company",958,"cubic inches",18.3,30.8,0.9,1.7,0.3,0.41,5.5,5.4,0.13,0.15,0.3,0.41,0.3,0.41,{"v":33750,"d":"33,750"}]
["5ECTK0668ge1","Reman","EcoTrans Environmental, Inc",668,"cubic inches",18,47,2.5,2.7,null,null,9.1,10.1,0.31,0.34,0.74,0.86,null,null,{"v":30750,"d":"30,750"}]
["5GETK0958EFF","Reman","Transportation Systems Business Operations of General Electric Company",958,"cubic inches",17.45,25.45,0.4,0.6,0.2,0.2,5.1,5.8,0.14,0.23,0.2,0.3,0.2,0.3,{"v":33750,"d":"33,750"}]
["6getg0958efb","Fresh","Transportation Systems Business Operations of General Electric Company",958,"cubic inches",9.2,14.2,0.4,0.6,0.16,0.27,5.3,5.9,0.1,0.13,0.16,0.27,0.16,0.27,{"v":33750,"d":"33,750"}]
["6GETK0958EFF","Reman","Transportation Systems Business Operations of General Electric Company",958,"cubic inches",17.45,25.45,0.4,0.6,0.2,0.2,5.1,5.8,0.14,0.23,0.2,0.3,0.2,0.3,{"v":33750,"d":"33,750"}]
["6GETK0958EFB","Reman","Transportation Systems Business Operations of General Electric Company",958,"cubic inches",9.8,15.1,0.9,1.7,0.3,0.41,5.5,5.4,0.13,0.15,0.3,0.41,0.3,0.41,{"v":33750,"d":"33,750"}]
["6GETK0668EFB","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",26.2,36.2,1,1.3,0.41,0.65,7.8,10.4,0.26,0.41,0.41,0.65,0.41,0.65,{"v":33750,"d":"33,750"}]
["6GETK0668EFF","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",25.3,30.4,1,1.2,0.31,0.5,7,10.2,0.17,0.28,0.31,0.5,0.31,0.5,{"v":33750,"d":"33,750"}]
["6GETK0668EFD","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",16.7,27.6,0.9,1.2,0.39,0.64,8.7,11.2,0.17,0.29,0.39,0.64,0.4,0.67,{"v":33750,"d":"33,750"}]
["6GETK0668EFA","Reman","Transportation Systems Business Operations of General Electric Company",688,"cubic inches",21.8,33.2,1.7,2.4,0.55,0.77,9,11.6,0.42,0.49,0.55,0.77,0.55,0.77,{"v":30750,"d":"30,750"}]
["6GETK0668MFA","Reman","Transportation Systems Business Operations of General Electric Company",688,"cubic inches",33,40,2.5,4.1,0.84,1.51,9.1,11.5,0.45,0.56,0.84,1.51,0.84,1.51,{"v":33750,"d":"33,750"}]
["6GETK0959EFB","Reman","Transportation Systems Business Operations of General Electric Company",959,"cubic inches",32,40,1.2,1.8,0.48,0.84,7.9,8.8,0.34,0.46,0.48,0.84,0.48,0.84,{"v":46875,"d":"46,875"}]
["6GETK0668EPC","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",30.2,40.9,0.9,1.5,0.4,0.68,9,11.7,0.17,0.29,0.4,0.68,0.4,0.68,{"v":31875,"d":"31,875"}]
["6getk0645mfa","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",23,34,3.2,3.5,0.9,1.43,10,12.5,0.48,0.65,0.9,1.43,0.9,1.43,null,{"v":750000,"d":"750,000"}]
["6GETK0645MSA","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",26.1,32,null,4.1,null,2.08,null,12.3,null,0.66,null,2.08,null,2.08,null,{"v":750000,"d":"750,000"}]
["6GETK0645MFC","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",22.2,38.2,2.5,2.3,0.86,1.23,9.1,11.3,0.55,0.56,0.86,1.23,0.86,1.23,null,{"v":750000,"d":"750,000"}]
["6GETK0645MFE","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",20.9,30.7,1.8,2.2,0.57,0.83,10.5,12.9,0.37,0.38,0.57,0.83,0.57,0.83,null,{"v":750000,"d":"750,000"}]
["6GETK0710MFA","Reman","Transportation Systems Business Operations of General Electric Company",710,"cubic inches",23.7,26.6,4.2,2.5,0.72,1.15,11.1,15.2,0.38,0.37,0.72,1.15,0.72,1.15,null,{"v":750000,"d":"750,000"}]
["6GETK0710MFC","Reman","Transportation Systems Business Operations of General Electric Company",710,"cubic inches",19.2,23.5,2.5,1.2,0.44,0.72,8.9,12.4,0.31,0.26,0.44,0.72,0.44,0.72,null,{"v":750000,"d":"750,000"}]
["6GETK0710MFE","Reman","Transportation Systems Business Operations of General Electric Company",710,"cubic inches",16.3,20,2.7,1.2,0.45,0.76,10.2,14.5,0.31,0.25,0.45,0.76,0.45,0.76,null,{"v":750000,"d":"750,000"}]
["5GETK0645MST","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",19.5,26.5,null,4.1,null,1.74,null,7.8,null,0.53,null,1.74,null,1.74,null,{"v":750000,"d":"750,000"}]
["6ADGK0645EB3","Reman","Advanced Global Environmental, Inc.",645,"cubic inches",21,45,1.2,1.9,null,null,9,11.7,0.52,0.48,0.86,1.38,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6GETK0959EFC","Reman","Transportation Systems Business Operations of General Electric Company",959,"cubic inches",31.1,40.3,1,1.5,0.51,0.81,9.3,11.4,0.28,0.41,0.51,0.81,0.1,0.16,{"v":46875,"d":"46,875"}]
["6NREGCM19LOC","Fresh","National Railway Equipment Company",3.17,"liters",9.27,8.73,0.9,1.5,0,0,2.8,3.4,0.03,0.06,0.02,0.04,0,0,{"v":10275,"d":"10,275"}]
["6GETK0645MST","Reman","Transportation Systems Business Operations of General Electric Company",645,"cubic inches",19.5,26.5,null,4.1,null,1.74,null,7.8,null,0.53,null,1.74,null,1.74,null,{"v":750000,"d":"750,000"}]
["6EMDK0710ES1","Reman","Electro-Motive Diesel, Inc.",710,"cubic inches",32.545,46.99,1.8,1.4,null,null,9.2,9.8,0.33,0.36,0.5,0.77,null,null,{"v":30000,"d":"30,000"}]
["6EMDK0645EBL","Reman","Electro-Motive Diesel, Inc.",645,"cubic inches",28.335,38.85,4.5,2.3,null,null,10.9,11.6,0.47,0.41,0.41,0.84,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6EMDK0710MJA","Reman","Electro-Motive Diesel, Inc.",710,"cubic inches",13.855,30.83,1.6,0.9,null,null,7.8,9.1,0.52,0.32,0.68,0.82,null,null,{"v":22500,"d":"22,500"}]
["6EMDK0645EAL","Reman","Electro-Motive Diesel, Inc.",645,"cubic inches",25.995,40.36,4.7,2.4,null,null,8.1,8.3,0.54,0.45,0.44,0.96,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6EMDK0710MJ0","Reman","Electro-Motive Diesel, Inc.",710,"cubic inches",14.545,18.98,1.6,0.8,null,null,8.9,10.6,0.3,0.26,0.5,0.84,null,null,{"v":28500,"d":"28,500"}]
["6EMDK16.5ES2","Reman","Electro-Motive Diesel, Inc.",16.55,"liters",14.845,31.66,1.9,1.4,null,null,8,8.4,0.26,0.27,0.74,1.24,null,null,{"v":45000,"d":"45,000"}]
["6EMDK0710EJ0","Reman","Electro-Motive Diesel, Inc.",710,"cubic inches",22.205,32.06,1.5,1.3,null,null,8.6,8.7,0.29,0.33,0.43,0.61,null,null,{"v":30000,"d":"30,000"}]
["6EMDG0710ES1","Fresh","Electro-Motive Diesel, Inc.",710,"cubic inches",11.955,26.32,0.9,0.6,null,null,5,6.4,0.11,0.18,0.17,0.31,null,null,{"v":32250,"d":"32,250"}]
["6NREK0645ENP","Reman","National Railway Equipment Co.",645,"cubic inches",22.1,22.2,2.6,2.2,0,0,9.1,11,0.54,0.62,0.26,0.23,0,0,null,{"v":750000,"d":"750,000"}]
["6CSXK0710ES6","Reman","CSXT Environmental Corporation",710,"cubic inches",21.7,28.9,1.4,1.2,null,null,8.4,8.7,0.32,0.36,0.83,0.99,null,null,{"v":37500,"d":"37,500"}]
["6CSXK0710ES2","Reman","CSXT Environmental Corporation",710,"cubic inches",16.7,21.9,1.1,1.5,null,null,8.7,8.9,0.33,0.34,0.86,0.99,null,null,{"v":30750,"d":"30,750"}]
["6CSXK0710EC2","Reman","CSXT Environmental Corporation",710,"cubic inches",25.5,48.5,1.6,1.7,null,null,8.8,8.7,0.56,0.45,0.94,0.89,null,null,{"v":30750,"d":"30,750"}]
["6CSXK0710GB3","Reman","CSXT Environmental Corporation",710,"cubic inches",11.5,18,1.3,1,null,null,9.2,13.4,0.37,0.38,0.92,1.11,null,null,{"v":30750,"d":"30,750"}]
["6CSXK0710GB0","Reman","CSXT Environmental Corporation",710,"cubic inches",29.5,40,2.3,1.5,null,null,8.6,10.6,0.41,0.52,0.96,1.14,null,null,{"v":29250,"d":"29,250"}]
["6CSXK0645F3X","Reman","CSXT Environmental Corporation",645,"cubic inches",12.5,16,1.9,1.6,null,null,8.6,9.9,0.41,0.4,0.9,1.07,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6CSXK0645E3Z","Reman","CSXT Environmental Corporation",645,"cubic inches",11.5,14,1.1,1.3,null,null,9,11.6,0.37,0.39,0.91,1.15,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6CSXK0645E3Y","Reman","CSXT Environmental Corporation",645,"cubic inches",11.5,16,1,1.4,null,null,8.8,10,0.39,0.4,0.93,1.13,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6CSXK0645E3X","Reman","CSXT Environmental Corporation",645,"cubic inches",20.5,29,1.2,1.5,null,null,8.8,10.1,0.42,0.44,0.96,1.18,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6CSXK0645E3W","Reman","CSXT Environmental Corporation",645,"cubic inches",16.5,35,1.7,1.7,null,null,8.1,9.3,0.39,0.39,0.94,1.13,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6CSXK0645E21","Reman","CSXT Environmental Corporation",645,"cubic inches",7.5,12,0,1.4,null,null,0,12.4,0,0.29,0,1.38,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6CSXK0645EC2","Reman","CSXT Environmental Corporation",645,"cubic inches",16.4,27.8,0,1.6,null,null,0,12.6,0,0.38,0,1.89,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6CSXK0645E02","Reman","CSXT Environmental Corporation",645,"cubic inches",11.5,18,0,2.7,null,null,0,12.5,0,0.49,0,1.46,{"$nulls":3},{"v":750000,"d":"750,000"}]
["6ECTK0668ge1","Reman","EcoTrans Environmental, Inc",668,"cubic inches",18,47,2.5,2.7,null,null,9.1,10.1,0.31,0.34,0.74,0.86,null,null,{"v":30750,"d":"30,750"}]
["6RHTk0121BD1","Reman","RailPower Hybrid Technologies, Corp.",121,"cubic inches",18.8,24.8,null,1.1,{"$nulls":3},5,null,0.15,null,0.27,null,null,{"v":15750,"d":"15,750"}]
["6NREK0645ERT","Reman","National Railway Equipment Company",645,"cubic inches",24.7,24.3,null,5.8,null,0,null,6.1,null,0.45,null,0.91,{"$nulls":3},{"v":750000,"d":"750,000"}]
["5mpik1645f3b","Reman","Motive Power",645,"cubic inches",null,null,1.7,2,0.47,0.71,6.8,9.7,0.4,0.46,0.47,0.71,0.47,0.71,{"v":27000,"d":"27,000"},{"v":750000,"d":"750,000"}]
["5GETK0668EPC","Reman","Transportation Systems Business Operations of General Electric Company",668,"cubic inches",30.2,40.9,0.9,1.5,0.4,0.68,9,11.7,0.17,0.29,0.4,0.68,0.4,0.68,{"v":31875,"d":"31,875"}]
["5GMXG0710ES3","Fresh","General Motors Electro-Motive Division",710,"cubic inches",19.655,33.26,1.1,0.8,null,null,6.8,7.4,0.14,0.2,0.27,0.41,null,null,{"v":30000,"d":"30,000"}]