{"text_format":"3","workbook":"xlsx","n_sheets":11,"sheets":["readme&changelog","Fireplace Calculator","Woodstove PM Calculator","Woodstove worksheet","Example Woodstove worksheet","References","cordwood_density","cordwood-burnrate","dropdown","pellet-burnrate","NEI-activity_data"],"not_rendered":{"images":1,"defined_names":77,"pivot_tables":2},"read":"whole","date_system":"1900"}

{"sheet":"readme&changelog","index":0,"n_rows":28,"n_cols":2,"rows_kept":28}
["EPA Residential Wood Combustion (RWC) Emissions Calculator"]
[]
["Tab","Description"]
["Fireplace Calculator","Contains Instructions and computations for emission reductions for PM and other pollutants by retrofitting fireplace to a gas or electric appliance"]
[]
["Woodstove PM  Calculator","Contains Instructions and computations for PM emission reductions from changeouts or retrofits of wood burning room heater appliances.  Summarizes data provided in the Woodstove worksheet."]
[]
["Woodstove worksheet","Users provide input parameters for each changeout or retrofit in this worksheet.  Contains emissions calculations for PM2.5 for each change out (pre- and post-change out)"]
[]
["References","Provides defaults for input parameters and references and/or methodology.  Includes emission factor (EF) and efficiency defaults, where available"]
[]
["cordwood_density","County-specific default data for cordwood densities based on the 2017 NEI approaches (see References TAB for more details)"]
[]
["cordwood_burnrate","County-specific default data for amount of wood burned per year per appliance type,  based on the 2017 NEI approaches (see References TAB for more details). Result of Pivot Table of \"NEI-activity_data\" TAB"]
[]
["Example Woodstove worksheet","Provides example of populated Woodstove worksheet"]
[]
["dropdown","Used by the Woodstove worksheet. Allowable values of \"Old Device Type\" and \"New Device Type\""]
[]
["pellet-burnrate","Not used"]
[]
["NEI-activity_data","NEI Wagon Wheel Tool Activity data used to compute the values in the burnrate TABs.  Developed as follows:  1) Used WagonWheel tool from the 2017 NEI.  2) Ran WagonWheel Tool for all states for RWC sector. 3) Created TAB \"NEI ACTIVITY DATA\" by running Query 8 Distribution to SCCs (in the module \"RWC\")."]
[]
[]
["CHANGELOG"]
["Date","Change"]
["2021-05-03","First Version"]
["2021-07-28","Pre-2015 certified stove is changed to \"Certified-20 years or older\" and the \"Example Woodstove worksheet\" is changed to include only \"Uncertified\" as the the \"Old Device Type\".  Added more values after decimal place in Woodstove PM Calculator and Fireplace Calculator TABs"]

{"sheet":"Fireplace Calculator","index":1,"n_rows":59,"n_cols":9,"rows_kept":59}
["Fireplace Calculator ---- Directions for use:"]
["1) Review and/or revise the wood density and cords of wood burned per year values (cells B8 and E8; cells B10 and E10). "]
["2) Enter number of fireplaces changed to gas or electric (cell B9)"]
["3) Optional:  Review / revise fireplace emission factor default values provided in column G if you have more specific data"]
["4) Scroll below for calculated emission reductions"]
[]
["Parameters for Calculation of Open Fireplace Retrofit Benefit","Inputs","Input Description","Basis of Default value","Basis of User value (User Please fill in)"]
["Wood density to convert cords to tons (tons oven dried wood/cord) = ",1.03,"use appropriate wood density (tons/cord) or choose county-level default from the tab labelled \"density tons-per-cord\"","2017 NEI Wagon-Wheel - RWC module; 1.03 is the value for Autuaga County, AL (FIPS 01001)","used default for Autuaga County, AL"]
["# of Fireplaces changed to gas or electric appliances = ",8,"input # of FP's being retrofitted (assume all go to gas or electric heaters)"]
["Burnrate for heating (cords/unit/yr) = ",0.19,"use appropriate burnrate or choose county-level, fireplace default from the tab labeled \"cordwood-burnrate\" (Fireplace burnrate is column D in that worksheet)","2017 NEI Wagon-Wheel - RWC module; 0.19 is the value for Autuaga County, AL (FIPS 01001)","used default for Autuaga County, AL"]
[null," "]
[" ",{"$nulls":4},"Criteria Pollutant/Precursor (CAP)","Emission factors for Fireplaces(lb/ton)","Reference"]
[" ",{"$nulls":3}," ","CO",149,"Houck, J.E. and B.N. Eagle. 2006. Task 6 Technical Memorandum 4 (Final Report): Control Analysis and Documentation for Residential Wood Combustion in the MANE-VU Region. Prepared for MARAMA. Table 3.03:  74.6 g/kg (https://s3.amazonaws.com/marama.org/wp-content/uploads/2019/09/13093812/RWC_FinalReport_121906.pdf)"]
[" ",{"$nulls":3}," ","SO2",0.4,"U.S. Environmental Protection Agency. 1996. AP-42, Fifth Edition, Chapter 1 External Combustion Sources, Sections 1.9 Residential Fireplaces and 1.10 Residential Wood Stove. (https://www.epa.gov/sites/production/files/2020-09/documents/1.9_residential_fireplaces.pdf)"]
[" ",{"$nulls":4},"NOX",2.6,"U.S. Environmental Protection Agency. 1996. AP-42, Fifth Edition, Chapter 1 External Combustion Sources, Sections 1.9 Residential Fireplaces and 1.10 Residential Wood Stove. (https://www.epa.gov/sites/production/files/2020-09/documents/1.9_residential_fireplaces.pdf)"]
[" ",{"$nulls":3}," ","VOC",18.9,"Houck, J.E. and B.N. Eagle. 2006. Task 6 Technical Memorandum 4 (Final Report): Control Analysis and Documentation for Residential Wood Combustion in the MANE-VU Region. Prepared for MARAMA. Table 3.03 9.43 g/kg (https://s3.amazonaws.com/marama.org/wp-content/uploads/2019/09/13093812/RWC_FinalReport_121906.pdf)"]
[{"$nulls":5},"PM2.5-PRI",23.6,"Houck, 2001: Houck, 2001:   Houck, J.E., J. Crouch, and R.H. Huntley. 2001. Review of Wood Heater and Fireplace Emission Factors. Technical presentation at the International Emission Inventory Conference. Denver, CO.  Table 3, use mean value of 11.8 g/ dry kg Available at: http://www.bioenergylists.org/stovesdoc/Environment/houck.pdf or ftp://newftp.epa.gov/air/nei/ei_conference/EI10/pm/houck.pdf "]
[null,"Emission Reduction (tons)",{"$nulls":3},"PM10-PRI",23.6,"Houck, 2001: Houck, 2001:   Houck, J.E., J. Crouch, and R.H. Huntley. 2001. Review of Wood Heater and Fireplace Emission Factors. Technical presentation at the International Emission Inventory Conference. Denver, CO.  Table 3, use mean value of 11.8 g/ dry kg Available at: http://www.bioenergylists.org/stovesdoc/Environment/houck.pdf or ftp://newftp.epa.gov/air/nei/ei_conference/EI10/pm/houck.pdf "]
[null,"Pollutant","Total Emissions Avoided",null,null,"NH3",23.6,"Houck, J.E. and B.N. Eagle. 2006. Task 6 Technical Memorandum 4 (Final Report): Control Analysis and Documentation for Residential Wood Combustion in the MANE-VU Region. Prepared for MARAMA. Table 3.03:  74.6 g/kg (https://s3.amazonaws.com/marama.org/wp-content/uploads/2019/09/13093812/RWC_FinalReport_121906.pdf)"]
[null,"CO",{"$f":"(Numb_FP*EF_CO*cords_tons*Burnrate)/2000","v":{"v":0.11663720000000001,"d":"0.1166"}}]
[null,"SO2",{"$f":"(Numb_FP*EF_SO2*cords_tons*Burnrate)/2000","v":{"v":0.00031312,"d":"0.0003"}},null,"HAP Pollutant Code","HAP Name","HAP to CAP ratio","CAP used","Reference"]
[null,"NOX",{"$f":"(Numb_FP*EF_NOX*cords_tons*Burnrate)/2000","v":{"v":2.03528E-3,"d":"0.0020"}},null,120127,"Anthracene",0.0002502107,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"VOC",{"$f":"(Numb_FP*EF_VOC*cords_tons*Burnrate)/2000","v":{"v":0.01479492,"d":"0.0148"}},null,2531842,"2-Methylphenanthrene",1.352883E-4,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"PM2.5-PRI",{"$f":"(Numb_FP*EF_PM25*cords_tons*Burnrate)/2000","v":{"v":0.018474080000000004,"d":"0.0185"}},null,100414,"Ethyl Benzene",1.6656466E-3,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"PM10-PRI",{"$f":"(Numb_FP*G18*cords_tons*Burnrate)/2000","v":{"v":0.018474080000000004,"d":"0.0185"}},null,106990,"1,3-Butadiene",0.0085100719,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"HAP Reductions (tons)",null,null,107028,"Acrolein",0.0045823464,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,{"$f":"F22","v":"Anthracene"},{"$f":"VOCemis*VLOOKUP(B27,F:G,2,FALSE)","v":{"v":3.701847289644e-06,"d":"3.702E-06"}},null,108383,"m-Xylene",0.004364139,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"2-Methylphenanthrene",{"v":2.001579575436e-06,"d":"2.002E-06"},null,108883,"Toluene",0.0114922339,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Ethyl Benzene",{"v":2.4643108195272e-05,"d":"2.464E-05"},null,108952,"Phenol",0.0381862202,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"1,3-Butadiene",{"v":1.2590583295474798E-4,"d":"1.259E-04"},null,50000,"Formaldehyde",0.084737041,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Acrolein",{"v":6.7795448400288007E-5,"d":"6.780E-05"},null,123386,"Propionaldehyde",0.0185475927,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"m-Xylene",{"v":6.456708737388e-05,"d":"6.457E-05"},null,1319773,"Cresol/Cresylic Acid (Mixed Isomers)",0.0341566647,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Toluene",{"v":0.000170026681171788,"d":"1.700E-04"},null,123319,"Hydroquinone",0.0012510533,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Phenol",{"v":0.000564962072961384,"d":"5.650E-04"},null,832699,"1-Methylphenanthrene",0.0001614732,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Formaldehyde",{"v":0.00125367774263172,"d":"1.254E-03"},null,85018,"Phenanthrene",1.1419498E-3,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Propionaldehyde",{"v":0.000274410150189084,"d":"2.744E-04"},null,86737,"Fluorene",3.229463E-4,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Cresol/Cresylic Acid (Mixed Isomers)",{"v":0.000505345121703324,"d":"5.053E-04"},null,90120,"1-Methylnaphthalene",0.000770998,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Hydroquinone",{"v":1.8509233489235997E-5,"d":"1.851E-05"},null,91203,"Naphthalene",0.0165109942,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"1-Methylphenanthrene",{"v":2.3889830761439998E-6,"d":"2.389E-06"},null,91576,"2-Methylnaphthalene",0.0010910349,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Phenanthrene",{"v":1.6895055935015998E-5,"d":"1.690E-05"},null,95476,"o-Xylene",0.001316515,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Fluorene",{"v":4.777964672796e-06,"d":"4.778E-06"},null,98862,"Acetophenone",0.0002836691,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"1-Methylnaphthalene",{"v":1.1406853730159999E-5,"d":"1.141E-05"},null,206440,"Fluoranthene",2.218438E-4,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Naphthalene",{"v":0.000244278838309464,"d":"2.443E-04"},null,208968,"Acenaphthylene",0.0013528832,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"2-Methylnaphthalene",{"v":1.6141774062707998E-5,"d":"1.614E-05"},null,120809,"Catechol",0.0226935251,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[" ","o-Xylene",{"v":1.94777341038e-05,"d":"1.948E-05"},null,129000,"Pyrene",0.0001360157,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Acetophenone",{"v":4.196861640972e-06,"d":"4.197E-06"},null,75070,"Acetaldehyde",0.1239415603,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Fluoranthene",{"v":3.2821612734959997E-6,"d":"3.282E-06"},null,203123,"Benzo(g,h,i)Fluoranthene",5.9643239e-06,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Acenaphthylene",{"v":2.0015798713344003E-5,"d":"2.002E-05"},null,83329,"Acenaphthene",1.46926E-4,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Catechol",{"v":0.000335748888372492,"d":"3.357E-04"},null,71432,"Benzene",0.0278577568,"VOC","Emissions Inventory System, HAP augmentation, computed from SPECIATE database profile 4642 as weight %/100 * TOG-to-VOC ratio .  Schauer, J.J., M.J. Kleeman, G.R. Cass, and B.R.T. Simoneit. 2001.  'Measurement of Emissions from Air Pollution Sources. 3. C1-C29 Organic Compounds from Fireplace Combustion of Wood',  Environmental Science and Technology, vol. 35, no. 9:1716-1728. http://doi.org/10.1021/es001331e "]
[null,"Pyrene",{"v":2.012341400244e-06,"d":"2.012E-06"},null,50328,"Benzo[a]Pyrene",{"$f":"0.00074/EF_VOC","v":{"v":3.9153439153439155E-5,"d":"3.92E-05"}},"VOC","Houck, J.E. and B.N. Eagle. 2006. Task 6 Technical Memorandum 4 (Final Report): Control Analysis and Documentation for Residential Wood Combustion in the MANE-VU Region. Prepared for MARAMA. (https://s3.amazonaws.com/marama.org/wp-content/uploads/2019/09/13093812/RWC_FinalReport_121906.pdf)  Use Table 3.03 value of 0.37 mg/kg (.00074 lb/ton) and divide by VOC  EF of  18.9 lb/ton to get"]
[null,"Acetaldehyde",{"v":1.833705469313676E-3,"d":"1.834E-03"},null,7439976,"Mercury",{"$f":"0.0000154/EF_PM25","v":{"v":6.52542372881356e-07,"d":"6.53E-07"}},"PM2.5","See cell C54 (Mercury Notes)"]
[null,"Benzo(g,h,i)Fluoranthene",{"v":8.8241694954587992E-8,"d":"8.824E-08"}]
[null,"Acenaphthene",{"v":2.17375841592E-6,"d":"2.174E-06"}]
[null,"Benzene",{"v":0.000412153283235456,"d":"4.122E-04"}]
[null,"Benzo[a]Pyrene",{"v":5.79272e-07,"d":"5.793E-07"}]
[null,"Mercury",{"$f":"PM25emis*VLOOKUP(B56,F:G,2,FALSE)","v":{"v":1.2055120000000003E-8,"d":"1.206E-08"}}]
[]
["* NOTES ON MERCURY MULTIPLICATION FACTOR"]
["Use Hg concentration in wood, assume it is all emitted.  That assumption is  backed up by:  Jiaoyan Huang, Philip K. Hopke, Hyun-Deok Choi, James R. Laing, Huailue Cui, Tiffany J. Zananski, Sriraam Ramanathan Chandrasekaran, Oliver V. Rattigan, Thomas M. Holsen, “Mercury (Hg) emissions from domestic biomass combustion for space heating”, Chemosphere,Volume 84, Issue 11,2011,Pages 1694-1699,ISSN 0045-6535,https://doi.org/10.1016/j.chemosphere.2011.04.078.(http://www.sciencedirect.com/science/article/pii/S0045653511005091)\n\nFor the value, use this paper:  Concentrations and content of mercury in bark, wood, and leaves in hardwoods and conifers in four forested sites in the northeastern USA\nYang Y, Yanai RD, Driscoll CT, Montesdeoca M, Smith KT (2018) Concentrations and content of mercury in bark, wood, and leaves in hardwoods and conifers in four forested sites in the northeastern USA. PLOS ONE 13(4): e0196293. https://doi.org/10.1371/journal.pone.0196293.  The resultant factor is 15.4 E-6 lb/ton.  The ratio to PM2.5 is computed by dividing that by the PM2.5 EF."]

{"sheet":"Woodstove PM Calculator","index":2,"n_rows":30,"n_cols":8,"rows_kept":30}
["Woodstove PM Calculator ---- Directions for use:"]
["1) Review and revise the wood density and cords of wood burned per year values  (cells C13 and C14; cells E13 and E14).  "]
["          If you have home-specific wood burned per year values, you can enter them in the Woodstove Worksheet, column  B).  See \"Example Woodstove worksheet for an example\""]
["2) Enter the information noted in the heading for each highlighted column (columns A-F and H-M) for each change-out/retrofit in the Woodstove Worksheet.  You can enter up to 999 rows. "]
["          See the  \"Example Woodstove worksheet\" for an example. "]
["3) We provide defaults for Efficiency, Uncertified Stove Emission Factor (EF), Non-wood option EF and the Pellet (EF)- -- see References"]
["4) This calculator does not provide a default EF for the different types of certified stoves: certified-20 years or older, hybrid, catalytic, non-catalytic due to a lack of data at this time.  If you are an agency trying to determine emission factors and have questions feel free to contact Larry Brockman, brockman.larry@epa.gov."]
[]
[]
["A Summary and Emissions Reductions for PM are provided below"]
[]
["Default Stove Usage (Burn rate and Cordwood Density) Parameters for Calculation of WS Changeout Benefit","Input Instruction","Inputs","Basis of Default value (see References TAB) for detail","Basis of User value (User Please fill in)"]
["Wood density to convert cords to tons (tons oven dried wood/cord) = ","Use local data or choose county-level default from \"cordwood_density\" TAB",1.03," 1.03 cords/ton is the value for Autuaga County, AL (FIPS 01001)","used default for Autuaga County, AL"]
["Cords of Wood Burned per Woodstove per year = ","Use local data or choose county-leve default from \"cordwood-burnrate\" TAB",0.54,"0.54 cords/year is the value for Autuaga County, AL (FIPS 01001)","used default for Autuaga County, AL"]
[]
["Summary of Change-outs based on the Information in the Woodstove worksheet"]
["OLD STOVE TYPE   to CHANGEOUT TYPE","NON-WOOD OPTION (include removal with no replacement)","PELLET","CERTIFIED HYBRID","CERTIFED CATALYTIC","CERTIFIED NONCAT"]
["UNCERTIFIED",{"$f":"COUNTIFS('Woodstove worksheet'!D2:D999,\"Uncertified\",'Woodstove worksheet'!I2:I999,dropdown!C5)","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!D2:D999,\"Uncertified\",'Woodstove worksheet'!I2:I999,\"Pellet\")","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!D2:D999,\"Uncertified\",'Woodstove worksheet'!I2:I999,\"Hybrid\")","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!$D$2:$D$999,\"Uncertified\",'Woodstove worksheet'!$I$2:$I$999,\"Catalytic\")","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!$D$2:$D$999,\"Uncertified\",'Woodstove worksheet'!$I$2:$I$999,\"Non-catalytic\")","v":0}]
["CERTIFIED-20 YEARS OR OLDER",{"$f":"COUNTIFS('Woodstove worksheet'!D2:D999,\"Certified-20 years or older\",'Woodstove worksheet'!I2:I999,dropdown!C5)","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!D2:D999,\"Certified-20 years or older\",'Woodstove worksheet'!I2:I999,\"Pellet\")","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!D2:D999,\"Certified-20 years or older\",'Woodstove worksheet'!I2:I999,\"Hybrid\")","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!$D$2:$D$999,\"Certified-20 years or older\",'Woodstove worksheet'!$I$2:$I$999,\"Catalytic\")","v":0},{"$f":"COUNTIFS('Woodstove worksheet'!$D$2:$D$999,\"Certified-20 years or older\",'Woodstove worksheet'!$I$2:$I$999,\"Non-catalytic\")","v":0}]
[" "]
["Calculations (Before Changeout, by appliance; After Changeout, by type and Total Emisssions Avoided)"]
["BEFORE CHANGE-OUT APPLIANCES","PM Emissions (tons) Before Changeout",null,"AFTER CHANGE OUT APPLIANCES","PM Emissions (tons) [assume it is all PM2.5] After Changeout"]
["uncertified",{"$f":"SUMIF('Woodstove worksheet'!$D$2:$D$999,\"Uncertified\",'Woodstove worksheet'!$G$2:$G$999)","v":{"v":0,"d":"0.0000"}},null,"Non-Wood",{"$f":"SUMIF('Woodstove worksheet'!$I$2:$I$999,\"Non-wood\",'Woodstove worksheet'!$N$2:$N$999)","v":{"v":0,"d":"0.0000"}}]
["Certified-20 years or older",{"$f":"SUMIF('Woodstove worksheet'!$D$2:$D$999,\"Certified-20 years or older\",'Woodstove worksheet'!$G$2:$G$999)","v":{"v":0,"d":"0.0000"}},null,"PELLET",{"$f":"SUMIF('Woodstove worksheet'!$I$2:$I$999,\"Pellet\",'Woodstove worksheet'!$N$2:$N$999)","v":{"v":0,"d":"0.0000"}}]
[{"$nulls":3},"CERTIFIED HYBRID",{"$f":"SUMIF('Woodstove worksheet'!$I$2:$I$999,\"Hybrid\",'Woodstove worksheet'!$N$2:$N$999)","v":{"v":0,"d":"0.0000"}}," "]
[{"$nulls":3},"CERTIFED CATALYTIC",{"$f":"SUMIF('Woodstove worksheet'!$I$2:$I$999,\"Catalytic\",'Woodstove worksheet'!$N$2:$N$999)","v":{"v":0,"d":"0.0000"}},null,null," "]
[{"$nulls":3},"CERTIFIED NONCAT",{"$f":"SUMIF('Woodstove worksheet'!$I$2:$I$999,\"Non-catalytic\",'Woodstove worksheet'!$N$2:$N$999)","v":{"v":0,"d":"0.0000"}}," "]
["TOTAL BEFORE CHANGEOUT",{"$f":"SUM(B23:B25)","v":{"v":0,"d":"0.0000"}},null,"TOTAL AFTER CHANGEOUT",{"$f":"SUM(E23:E27)","v":{"v":0,"d":"0.0000"}}]
[]
[{"$nulls":3},"TONS PM EMISSIONS AVOIDED",{"$f":"(B28-E28)","v":{"v":0,"d":"0.00000"}}]

{"sheet":"Woodstove worksheet","index":3,"n_rows":999,"n_cols":14,"rows_kept":999}
["Date Of Change-out","Cords of Wood Burned in Old Device Per Year (Change this value if you have more specific information for your area)","Old device detail --include manufacturer and model specifics and year of old stove, if known)","Old device type Enter or Choose from Dropdown Menu (Uncertified Or Certified-20 years or older)","Old Device Emissions Factor for PM (lb/ton) -See References TAB for Default","Old device Efficiency (%) - see References TAB for Default","Calculated Emissions - BEFORE (tons) DO NOT ENTER VALUE","New device detail --include manufacturer and model specifics)","New Device Choose from Dropdown Menu","New Device Emissions Factor for PM  (lb/ton)- see References TAB for Default","New Device Efficiency -  (%) -see References for Default","Explain basis for EF","Expain basis for Efficiency","Calculated Emissions - AFTER (tons) DO NOT ENTER VALUE"]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54}," ",{"$nulls":3},{"$f":"IF(F2=\"\",\"\",E2*Conversion*B2/2000)","v":""},{"$nulls":6},{"$f":"IF(K2=\"\",\"\",J2*F2/K2*B2/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},{"$f":"IF(F3=\"\",\"\",E3*Conversion*B3/2000)","v":""},{"$nulls":6},""]
[null,0.54,{"$nulls":4},{"$f":"IF(D4=\"\",\"\",E4*Conversion*B4/2000)","v":""},null,null," ",{"$nulls":3},""]
[null,0.54,{"$nulls":3}," ","",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},{"$f":"IF(D66=\"\",\"\",E66*Conversion*B66/2000)","v":""},{"$nulls":6},{"$f":"IF(K66=\"\",\"\",J66*F66/K66*B66/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},{"$f":"IF(D130=\"\",\"\",E130*Conversion*B130/2000)","v":""},{"$nulls":6},{"$f":"IF(K130=\"\",\"\",J130*F130/K130*B130/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},{"$f":"IF(D194=\"\",\"\",E194*Conversion*B194/2000)","v":""},{"$nulls":6},{"$f":"IF(K194=\"\",\"\",J194*F194/K194*B194/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},{"$f":"IF(D258=\"\",\"\",E258*Conversion*B258/2000)","v":""},{"$nulls":6},{"$f":"IF(K258=\"\",\"\",J258*F258/K258*B258/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},{"$f":"IF(D322=\"\",\"\",E322*Conversion*B322/2000)","v":""},{"$nulls":6},{"$f":"IF(K322=\"\",\"\",J322*F322/K322*B322/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},{"$f":"IF(D386=\"\",\"\",E386*Conversion*B386/2000)","v":""},{"$nulls":6},{"$f":"IF(K386=\"\",\"\",J386*F386/K386*B386/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},{"$f":"IF(D450=\"\",\"\",E450*Conversion*B450/2000)","v":""},{"$nulls":6},{"$f":"IF(K450=\"\",\"\",J450*F450/K450*B450/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},{"$f":"IF(D501=\"\",\"\",E501*Conversion*B501/2000)","v":""},{"$nulls":6},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K514=\"\",\"\",J514*F514/K514*B514/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K578=\"\",\"\",J578*F578/K578*B578/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K642=\"\",\"\",J642*F642/K642*B642/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K706=\"\",\"\",J706*F706/K706*B706/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K770=\"\",\"\",J770*F770/K770*B770/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K834=\"\",\"\",J834*F834/K834*B834/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K898=\"\",\"\",J898*F898/K898*B898/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K962=\"\",\"\",J962*F962/K962*B962/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]

{"sheet":"Example Woodstove worksheet","index":4,"n_rows":999,"n_cols":14,"rows_kept":999}
["Date Of Change-out","Cords of Wood Burned in Old Device Per Year (if you have more specific information for your area, replace value)","Old device detail --include manufacturer and model specifics and year of old stove, if known)","Old device type Enter or Choose from Dropdown Menu (Uncertified Or Certified Stove, 20 years or older)","Old Device Emissions Factor for PM (lb/ton) -See References TAB for Default","Old device Efficiency (%) - see References TAB for Default","Calculated Emissions - BEFORE (tons) DO NOT ENTER VALUE","New device detail --include manufacturer and model specifics)","New Device Choose from Dropdown Menu","New Device Emissions Factor for PM  (lb/ton)- see References TAB for Default","New Device Efficiency -  (%) -see References for Default","Explain basis for EF","Expain basis for Efficiency","Calculated Emissions - AFTER (tons) DO NOT ENTER VALUE"]
[null,0.74," ","Uncertified",30.6,54,{"$f":"IF(F2=\"\",\"\",E2*Conversion*B2/2000)","v":0.011661659999999999},null,"Pellet",4.2,68,"default","default",{"$f":"IF(K2=\"\",\"\",J2*F2/K2*B2/2000*Conversion)","v":1.2710805882352942E-3}]
[null,0.34,null,"Uncertified",30.6,54,{"$f":"IF(F3=\"\",\"\",E3*Conversion*B3/2000)","v":0.005358060000000001},null,"Pellet",4.2,68,"default","default",0.00058401]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},null,"Uncertified",30.6,54,{"$f":"IF(D4=\"\",\"\",E4*Conversion*B4/2000)","v":8.509860000000001E-3},null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",{"$f":"IF(K66=\"\",\"\",J66*F66/K66*B66/2000*Conversion)","v":0}]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,{"$f":"IF(D68=\"\",\"\",E68*Conversion*B68/2000)","v":8.509860000000001E-3},null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",{"$f":"IF(K130=\"\",\"\",J130*F130/K130*B130/2000*Conversion)","v":9.2754529411764723E-4}]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,{"$f":"IF(D132=\"\",\"\",E132*Conversion*B132/2000)","v":8.509860000000001E-3},null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Pellet",4.2,68,"default","default",9.2754529411764723E-4]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",{"$f":"IF(K194=\"\",\"\",J194*F194/K194*B194/2000*Conversion)","v":0}]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,{"$f":"IF(D196=\"\",\"\",E196*Conversion*B196/2000)","v":8.509860000000001E-3},null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,null,"Uncertified",30.6,54,8.509860000000001E-3,null,"Non-wood (gas or electric)",0,100,"default","default",0]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},"",{"$nulls":6},{"$f":"IF(K258=\"\",\"\",J258*F258/K258*B258/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},{"$f":"IF(D260=\"\",\"\",E260*Conversion*B260/2000)","v":""},{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},"",{"$nulls":6},{"$f":"IF(K322=\"\",\"\",J322*F322/K322*B322/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},{"$f":"IF(D324=\"\",\"\",E324*Conversion*B324/2000)","v":""},{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},"",{"$nulls":6},{"$f":"IF(K386=\"\",\"\",J386*F386/K386*B386/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},{"$f":"IF(D388=\"\",\"\",E388*Conversion*B388/2000)","v":""},{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":4},"",{"$nulls":6},{"$f":"IF(K450=\"\",\"\",J450*F450/K450*B450/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},{"$f":"IF(D452=\"\",\"\",E452*Conversion*B452/2000)","v":""},{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":4},"",{"$nulls":6},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K514=\"\",\"\",J514*F514/K514*B514/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K578=\"\",\"\",J578*F578/K578*B578/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K642=\"\",\"\",J642*F642/K642*B642/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K706=\"\",\"\",J706*F706/K706*B706/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K770=\"\",\"\",J770*F770/K770*B770/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K834=\"\",\"\",J834*F834/K834*B834/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K898=\"\",\"\",J898*F898/K898*B898/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,{"$f":"Cords_of_Wood_Burned_per_UncertWoodstove","v":0.54},{"$nulls":11},{"$f":"IF(K962=\"\",\"\",J962*F962/K962*B962/2000*Conversion)","v":""}]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]
[null,0.54,{"$nulls":11},""]

{"sheet":"References","index":5,"n_rows":29,"n_cols":6,"rows_kept":29}
["This worksheet provides references/methodology for default values provided."]
[]
["1. Burn Rates and Cordwood Densities"]
["Item","Developed From","TAB","Full References"," "]
["cordwood density","2017 NEI Wagon-Wheel - RWC module","cordwood_density"]
["cordwood burn rate","2017 NEI Wagon-Wheel - RWC module (see below for the Approach)","cordwood-burnrate","2017 NEI  Residential Wood Combustion Documentation and Wagon-Wheel  can be found at: https://gaftp.epa.gov/air/nei/2017/doc/supporting_data/nonpoint/Residential%20Wood%20Combustion_DRAFT.DOCX  and https://gaftp.epa.gov/air/nei/2017/doc/supporting_data/nonpoint/WagonWheel_4.27.20.zip  "]
[]
[]
["Burnrate Approach"]
["Used WagonWheel tool from the 2017 NEI.  Ran for all states for RWC sector."]
["Created TAB \"NEI-activity_data\" by running Query 8 Distribution to SCCs (in the module \"RWC\")"]
["Made separate pivot tables for fireplace/stove versus central furnaces, took average across similar stove types (cordwood stove/insert,pellet stove, fireplace, forced air furnace, hydronic heater)"]
[]
["2017 NEI Wagon-Wheel and RWC References"]
["Documentation:  2017 NEI Technical Support Document, Section 4.15 and https://gaftp.epa.gov/air/nei/2017/doc/supporting_data/nonpoint/Residential%20Wood%20Combustion_DRAFT.DOCX"]
["Wagon Wheel and RWC Module (MS ACCESS):  https://gaftp.epa.gov/air/nei/2017/doc/supporting_data/nonpoint/WagonWheel_4.27.20.zip  "]
[]
["2. DEFAULTS:  PM Emission Factor (EF) [Assume PM = PM10 = PM25] and Stove Efficiency Information"]
["Stove Type","Default PM EF (lb/ton)","Basis of Default EF (where provided))","Default Efficiency (%)","Basis of Default Efficiency value (where provided)"]
["Uncertified",30.6,"AP42_1996",54,"AP42_1996"]
["Certified-20 years or older"," "," ",68,"AP42_1996"]
["Non-wood",0,"Assumption; while gas and electric will have emissions associated, assume they are negligible for estimation of change out reductions",100,"Assumption - Value not used since using EF=0"]
["Pellet",4.2,"AP42_1996",68,"AP42_1996"]
["Certified Hybrid",{"$nulls":4}," "]
["Certified Catalytic",{"$nulls":4}," "]
["Certified Non-catalytic",{"$nulls":4}," "]
[]
["EF and Efficiency References for Defaults"]
["AP42_1996","AP-42:Table 1.10-1 for Emission Factors, Table 1.10-5 for Efficiencies, Vol. 1. CH1.10, Final Section - Supplement B, October 1996. https://www.epa.gov/air-emissions-factors-and-quantification/ap-42-fifth-edition-volume-i-chapter-1-external-0"]

{"sheet":"cordwood_density","index":6,"n_rows":3143,"n_cols":5,"rows_kept":3143}
["FIPS State and County Code","County","Postal Code","Default Density (tons/cord)","New Density (tons/cord) (same as Default unless S/L/T provided values to override default)"]
["01001","Autauga","AL",1.3062,1.3062]
["01003","Baldwin","AL",1.2411,1.2411]
["01005","Barbour","AL",1.2923,1.2923]
["01007","Bibb","AL",1.3513,1.3513]
["01009","Blount","AL",1.3483,1.3483]
["01011","Bullock","AL",1.2441,1.2441]
["01013","Butler","AL",1.2679,1.2679]
["01015","Calhoun","AL",1.338,1.338]
["01017","Chambers","AL",1.2087,1.2087]
["01019","Cherokee","AL",1.3571,1.3571]
["01021","Chilton","AL",1.2829,1.2829]
["01023","Choctaw","AL",1.2819,1.2819]
["01025","Clarke","AL",1.2798,1.2798]
["01027","Clay","AL",1.2878,1.2878]
["01029","Cleburne","AL",1.2247,1.2247]
["01031","Coffee","AL",1.2459,1.2459]
["01033","Colbert","AL",1.334,1.334]
["01035","Conecuh","AL",1.2796,1.2796]
["01037","Coosa","AL",1.3323,1.3323]
["01039","Covington","AL",1.3096,1.3096]
["01041","Crenshaw","AL",1.3039,1.3039]
["01043","Cullman","AL",1.2988,1.2988]
["01045","Dale","AL",1.2832,1.2832]
["01047","Dallas","AL",1.3305,1.3305]
["01049","De Kalb","AL",1.29,1.29]
["01051","Elmore","AL",1.2838,1.2838]
["01053","Escambia","AL",1.3182,1.3182]
["01055","Etowah","AL",1.2948,1.2948]
["01057","Fayette","AL",1.3005,1.3005]
["01059","Franklin","AL",1.3305,1.3305]
["01061","Geneva","AL",1.2303,1.2303]
["01063","Greene","AL",1.303,1.303]
["01065","Hale","AL",1.3693,1.3693]
["01067","Henry","AL",1.3643,1.3643]
["01069","Houston","AL",1.2134,1.2134]
["01071","Jackson","AL",1.4005,1.4005]
["01073","Jefferson","AL",1.3487,1.3487]
["01075","Lamar","AL",1.3055,1.3055]
["01077","Lauderdale","AL",1.4004,1.4004]
["01079","Lawrence","AL",1.2704,1.2704]
["01081","Lee","AL",1.1974,1.1974]
["01083","Limestone","AL",1.3527,1.3527]
["01085","Lowndes","AL",1.2814,1.2814]
["01087","Macon","AL",1.3544,1.3544]
["01089","Madison","AL",1.1841,1.1841]
["01091","Marengo","AL",1.2396,1.2396]
["01093","Marion","AL",1.309,1.309]
["01095","Marshall","AL",1.4183,1.4183]
["01097","Mobile","AL",1.2262,1.2262]
["01099","Monroe","AL",1.3081,1.3081]
["01101","Montgomery","AL",1.2799,1.2799]
["01103","Morgan","AL",1.4024,1.4024]
["01105","Perry","AL",1.2635,1.2635]
["01107","Pickens","AL",1.2734,1.2734]
["01109","Pike","AL",1.3257,1.3257]
["01111","Randolph","AL",1.2743,1.2743]
["01113","Russell","AL",1.2276,1.2276]
["01115","St Clair","AL",1.3657,1.3657]
["01117","Shelby","AL",1.3069,1.3069]
["01119","Sumter","AL",1.2983,1.2983]
["01121","Talladega","AL",1.3033,1.3033]
["01123","Tallapoosa","AL",1.2843,1.2843]
["01125","Tuscaloosa","AL",1.2955,1.2955]
["01127","Walker","AL",1.3648,1.3648]
["01129","Washington","AL",1.2876,1.2876]
["01131","Wilcox","AL",1.2989,1.2989]
["01133","Winston","AL",1.3079,1.3079]
["02013","Aleutians East","AK",1.0276,1.683]
["02016","Aleutians West","AK",1.0276,1.683]
["02020","Anchorage","AK",1.0276,1.683]
["02050","Bethel","AK",1.0276,1.683]
["02060","Bristol Bay","AK",1.0276,1.683]
["02068","Denali","AK",1.0276,1.683]
["02070","Dillingham","AK",1.0276,1.683]
["02090","Fairbanks North Star","AK",1.1272,1.683]
["02100","Haines","AK",1.0276,1.683]
["02105","Hoonah Angoon","AK",1.0276,1.683]
["02110","Juneau","AK",1.0276,1.683]
["02122","Kenai Peninsula","AK",1.0276,1.683]
["02130","Ketchikan Gateway","AK",1.0276,1.683]
["02150","Kodiak Island","AK",1.0276,1.683]
["02158","Kusilvak","AK",1.0276,1.683]
["02164","Lake and Peninsula","AK",1.0276,1.683]
["02170","Matanuska Susitna","AK",1.0276,1.683]
["02180","Nome","AK",1.0276,1.683]
["02185","North Slope","AK",1.0276,1.683]
["02188","Northwest Arctic","AK",1.0276,1.683]
["02195","Petersburg","AK",1.0276,1.683]
["02198","Prince of Wales-Hyder","AK",1.0351,1.683]
["02220","Sitka","AK",1.0276,1.683]
["02230","Skagway","AK",1.0276,1.683]
["02240","Southeast Fairbanks","AK",1.0276,1.683]
["02261","Valdez Cordova","AK",1.0276,1.683]
["02275","Wrangell","AK",1.0351,1.683]
["02282","Yakutat","AK",1.0276,1.683]
["02290","Yukon Koyukuk","AK",1.0276,1.683]
["04001","Apache","AZ",1.0055,1.0055]
["04003","Cochise","AZ",1.017,1.017]
["04005","Coconino","AZ",1.0185,1.0185]
["04007","Gila","AZ",1.0276,1.0276]
["04009","Graham","AZ",1.0276,1.0276]
["04011","Greenlee","AZ",1.0219,1.0219]
["04012","La Paz","AZ",1.0276,1.0276]
["04013","Maricopa","AZ",1.0176,1.0176]
["04015","Mohave","AZ",1.0171,1.0171]
["04017","Navajo","AZ",1.0276,1.0276]
["04019","Pima","AZ",1.017,1.017]
["04021","Pinal","AZ",1.0176,1.0176]
["04023","Santa Cruz","AZ",1.017,1.017]
["04025","Yavapai","AZ",1.0171,1.0171]
["04027","Yuma","AZ",1.0276,1.0276]
["05001","Arkansas","AR",1.2767,1.2767]
["05003","Ashley","AR",1.3307,1.3307]
["05005","Baxter","AR",1.4112,1.4112]
["05007","Benton","AR",1.4399,1.4399]
["05009","Boone","AR",1.4603,1.4603]
["05011","Bradley","AR",1.3251,1.3251]
["05013","Calhoun","AR",1.3008,1.3008]
["05015","Carroll","AR",1.4423,1.4423]
["05017","Chicot","AR",1.2768,1.2768]
["05019","Clark","AR",1.3193,1.3193]
["05021","Clay","AR",1.3881,1.3881]
["05023","Cleburne","AR",1.3349,1.3349]
["05025","Cleveland","AR",1.3249,1.3249]
["05027","Columbia","AR",1.3018,1.3018]
["05029","Conway","AR",1.2265,1.2265]
["05031","Craighead","AR",1.3477,1.3477]
["05033","Crawford","AR",1.3715,1.3715]
["05035","Crittenden","AR",1.2183,1.2183]
["05037","Cross","AR",1.4759,1.4759]
["05039","Dallas","AR",1.2942,1.2942]
["05041","Desha","AR",1.2335,1.2335]
["05043","Drew","AR",1.3309,1.3309]
["05045","Faulkner","AR",1.3911,1.3911]
["05047","Franklin","AR",1.4207,1.4207]
["05049","Fulton","AR",1.4436,1.4436]
["05051","Garland","AR",1.3365,1.3365]
["05053","Grant","AR",1.2821,1.2821]
["05055","Greene","AR",1.3477,1.3477]
["05057","Hempstead","AR",1.2742,1.2742]
["05059","Hot Spring","AR",1.3161,1.3161]
["05061","Howard","AR",1.3121,1.3121]
["05063","Independence","AR",1.4162,1.4162]
["05065","Izard","AR",1.4092,1.4092]
["05067","Jackson","AR",1.2022,1.2022]
["05069","Jefferson","AR",1.3976,1.3976]
["05071","Johnson","AR",1.4051,1.4051]
["05073","Lafayette","AR",1.2787,1.2787]
["05075","Lawrence","AR",1.4203,1.4203]
["05077","Lee","AR",1.5085,1.5085]
["05079","Lincoln","AR",1.4279,1.4279]
["05081","Little River","AR",1.4013,1.4013]
["05083","Logan","AR",1.3673,1.3673]
["05085","Lonoke","AR",1.2925,1.2925]
["05087","Madison","AR",1.4098,1.4098]
["05089","Marion","AR",1.4472,1.4472]
["05091","Miller","AR",1.3234,1.3234]
["05093","Mississippi","AR",0.924,0.924]
["05095","Monroe","AR",1.3521,1.3521]
["05097","Montgomery","AR",1.375,1.375]
["05099","Nevada","AR",1.3256,1.3256]
["05101","Newton","AR",1.4299,1.4299]
["05103","Ouachita","AR",1.3314,1.3314]
["05105","Perry","AR",1.3112,1.3112]
["05107","Phillips","AR",1.3217,1.3217]
["05109","Pike","AR",1.306,1.306]
["05111","Poinsett","AR",1.3714,1.3714]
["05113","Polk","AR",1.372,1.372]
["05115","Pope","AR",1.3583,1.3583]
["05117","Prairie","AR",1.2398,1.2398]
["05119","Pulaski","AR",1.3259,1.3259]
["05121","Randolph","AR",1.3929,1.3929]
["05123","St Francis","AR",1.4136,1.4136]
["05125","Saline","AR",1.269,1.269]
["05127","Scott","AR",1.4263,1.4263]
["05129","Searcy","AR",1.4439,1.4439]
["05131","Sebastian","AR",1.0948,1.0948]
["05133","Sevier","AR",1.3578,1.3578]
["05135","Sharp","AR",1.4496,1.4496]
["05137","Stone","AR",1.3793,1.3793]
["05139","Union","AR",1.3049,1.3049]
["05141","Van Buren","AR",1.4035,1.4035]
["05143","Washington","AR",1.4121,1.4121]
["05145","White","AR",1.361,1.361]
["05147","Woodruff","AR",1.4447,1.4447]
["05149","Yell","AR",1.3595,1.3595]
["06001","Alameda","CA",1.0276,1.0276]
["06003","Alpine","CA",1.0367,1.0367]
["06005","Amador","CA",1.0394,1.0394]
["06007","Butte","CA",1.0987,1.0987]
["06009","Calaveras","CA",1.0425,1.0425]
["06011","Colusa","CA",1.0276,1.0276]
["06013","Contra Costa","CA",1.0276,1.0276]
["06015","Del Norte","CA",1.2022,1.2022]
["06017","El Dorado","CA",1.0485,1.0485]
["06019","Fresno","CA",1.0276,1.0276]
["06021","Glenn","CA",1.017,1.017]
["06023","Humboldt","CA",1.0837,1.0837]
["06025","Imperial","CA",1.0276,1.0276]
["06027","Inyo","CA",1.017,1.017]
["06029","Kern","CA",1.0276,1.0276]
["06031","Kings","CA",1.0276,1.0276]
["06033","Lake","CA",1.0276,1.0276]
["06035","Lassen","CA",0.9579,0.9579]
["06037","Los Angeles","CA",1.0503,1.0503]
["06039","Madera","CA",1.0276,1.0276]
["06041","Marin","CA",1.0276,1.0276]
["06043","Mariposa","CA",1.0276,1.0276]
["06045","Mendocino","CA",1.0399,1.0399]
["06047","Merced","CA",1.0276,1.0276]
["06049","Modoc","CA",0.987,0.987]
["06051","Mono","CA",1.0276,1.0276]
["06053","Monterey","CA",1.0276,1.0276]
["06055","Napa","CA",1.0276,1.0276]
["06057","Nevada","CA",1.079,1.079]
["06059","Orange","CA",1.0304,1.0304]
["06061","Placer","CA",1.0256,1.0256]
["06063","Plumas","CA",0.9737,0.9737]
["06065","Riverside","CA",1.1136,1.1136]
["06067","Sacramento","CA",1.0276,1.0276]
["06069","San Benito","CA",1.0276,1.0276]
["06071","San Bernardino","CA",1.1047,1.1047]
["06073","San Diego","CA",1.0304,1.0304]
["06075","San Francisco","CA",1.0276,1.0276]
["06077","San Joaquin","CA",1.0276,1.0276]
["06079","San Luis Obispo","CA",1.0671,1.0671]
["06081","San Mateo","CA",1.0276,1.0276]
["06083","Santa Barbara","CA",1.0671,1.0671]
["06085","Santa Clara","CA",1.0276,1.0276]
["06087","Santa Cruz","CA",1.0276,1.0276]
["06089","Shasta","CA",1.0343,1.0343]
["06091","Sierra","CA",1.0192,1.0192]
["06093","Siskiyou","CA",1.0727,1.0727]
["06095","Solano","CA",1.0276,1.0276]
["06097","Sonoma","CA",1.0276,1.0276]
["06099","Stanislaus","CA",1.0276,1.0276]
["06101","Sutter","CA",1.0276,1.0276]
["06103","Tehama","CA",1.0141,1.0141]
["06105","Trinity","CA",1.0529,1.0529]
["06107","Tulare","CA",1.0359,1.0359]
["06109","Tuolumne","CA",0.9933,0.9933]
["06111","Ventura","CA",1.0671,1.0671]
["06113","Yolo","CA",1.0276,1.0276]
["06115","Yuba","CA",1.0486,1.0486]
["08001","Adams","CO",1.0276,1.0276]
["08003","Alamosa","CO",1.0188,1.0188]
["08005","Arapahoe","CO",1.0276,1.0276]
["08007","Archuleta","CO",1.0182,1.0182]
["08009","Baca","CO",1.0276,1.0276]
["08011","Bent","CO",1.0276,1.0276]
["08013","Boulder","CO",1.017,1.017]
["08014","Broomfield","CO",1.0276,1.0276]
["08015","Chaffee","CO",1.0179,1.0179]
["08017","Cheyenne","CO",1.0276,1.0276]
["08019","Clear Creek","CO",1.017,1.017]
["08021","Conejos","CO",1.0182,1.0182]
["08023","Costilla","CO",1.0577,1.0577]
["08025","Crowley","CO",1.0276,1.0276]
["08027","Custer","CO",1.017,1.017]
["08029","Delta","CO",1.0335,1.0335]
["08031","Denver","CO",1.0276,1.0276]
["08033","Dolores","CO",1.0581,1.0581]
["08035","Douglas","CO",1.017,1.017]
["08037","Eagle","CO",1.017,1.017]
["08039","Elbert","CO",1.0276,1.0276]
["08041","El Paso","CO",1.017,1.017]
["08043","Fremont","CO",1.017,1.017]
["08045","Garfield","CO",1.0582,1.0582]
["08047","Gilpin","CO",1.0276,1.0276]
["08049","Grand","CO",1.017,1.017]
["08051","Gunnison","CO",1.0579,1.0579]
["08053","Hinsdale","CO",1.0238,1.0238]
["08055","Huerfano","CO",1.017,1.017]
["08057","Jackson","CO",1.0587,1.0587]
["08059","Jefferson","CO",1.017,1.017]
["08061","Kiowa","CO",1.0276,1.0276]
["08063","Kit Carson","CO",1.0276,1.0276]
["08065","Lake","CO",1.0276,1.0276]
["08067","La Plata","CO",1.0135,1.0135]
["08069","Larimer","CO",1.0584,1.0584]
["08071","Las Animas","CO",1.0582,1.0582]
["08073","Lincoln","CO",1.0276,1.0276]
["08075","Logan","CO",1.017,1.017]
["08077","Mesa","CO",1.058,1.058]
["08079","Mineral","CO",1.0276,1.0276]
["08081","Moffat","CO",1.017,1.017]
["08083","Montezuma","CO",1.0526,1.0526]
["08085","Montrose","CO",1.0335,1.0335]
["08087","Morgan","CO",1.0276,1.0276]
["08089","Otero","CO",1.0276,1.0276]
["08091","Ouray","CO",1.0335,1.0335]
["08093","Park","CO",1.0579,1.0579]
["08095","Phillips","CO",1.0276,1.0276]
["08097","Pitkin","CO",1.017,1.017]
["08099","Prowers","CO",1.0276,1.0276]
["08101","Pueblo","CO",1.017,1.017]
["08103","Rio Blanco","CO",1.017,1.017]
["08105","Rio Grande","CO",1.0182,1.0182]
["08107","Routt","CO",1.017,1.017]
["08109","Saguache","CO",1.0258,1.0258]
["08111","San Juan","CO",1.0182,1.0182]
["08113","San Miguel","CO",1.0335,1.0335]
["08115","Sedgwick","CO",1.0276,1.0276]
["08117","Summit","CO",1.0276,1.0276]
["08119","Teller","CO",1.0276,1.0276]
["08121","Washington","CO",1.0276,1.0276]
["08123","Weld","CO",1.0276,1.0276]
["08125","Yuma","CO",1.0276,1.0276]
["09001","Fairfield","CT",1.4501,1.4501]
["09003","Hartford","CT",1.3604,1.3604]
["09005","Litchfield","CT",1.4219,1.4219]
["09007","Middlesex","CT",1.3562,1.3562]
["09009","New Haven","CT",1.4189,1.4189]
["09011","New London","CT",1.3539,1.3539]
["09013","Tolland","CT",1.3803,1.3803]
["09015","Windham","CT",1.4015,1.4015]
["10001","Kent","DE",1.252,1.252]
["10003","New Castle","DE",1.2987,1.2987]
["10005","Sussex","DE",1.1867,1.1867]
["11001","District of Columbia","DC",1.2934,1.2934]
["12001","Alachua","FL",1.4063,1.4063]
["12003","Baker","FL",1.3382,1.3382]
["12005","Bay","FL",1.2952,1.2952]
["12007","Bradford","FL",1.3694,1.3694]
["12009","Brevard","FL",1.2025,1.2025]
["12011","Broward","FL",1.2022,1.2022]
["12013","Calhoun","FL",1.3284,1.3284]
["12015","Charlotte","FL",1.017,1.017]
["12017","Citrus","FL",1.2822,1.2822]
["12019","Clay","FL",1.3009,1.3009]
["12021","Collier","FL",1.2906,1.2906]
["12023","Columbia","FL",1.2721,1.2721]
["12027","De Soto","FL",1.3305,1.3305]
["12029","Dixie","FL",1.3092,1.3092]
["12031","Duval","FL",1.3198,1.3198]
["12033","Escambia","FL",1.2627,1.2627]
["12035","Flagler","FL",1.1981,1.1981]
["12037","Franklin","FL",1.2149,1.2149]
["12039","Gadsden","FL",1.2553,1.2553]
["12041","Gilchrist","FL",1.216,1.216]
["12043","Glades","FL",1.3427,1.3427]
["12045","Gulf","FL",1.2249,1.2249]
["12047","Hamilton","FL",1.2371,1.2371]
["12049","Hardee","FL",1.4031,1.4031]
["12051","Hendry","FL",1.3173,1.3173]
["12053","Hernando","FL",1.2724,1.2724]
["12055","Highlands","FL",1.348,1.348]
["12057","Hillsborough","FL",1.3666,1.3666]
["12059","Holmes","FL",1.4744,1.4744]
["12061","Indian River","FL",1.1959,1.1959]
["12063","Jackson","FL",1.3486,1.3486]
["12065","Jefferson","FL",1.4001,1.4001]
["12067","Lafayette","FL",1.3064,1.3064]
["12069","Lake","FL",1.247,1.247]
["12071","Lee","FL",1.348,1.348]
["12073","Leon","FL",1.3656,1.3656]
["12075","Levy","FL",1.3517,1.3517]
["12077","Liberty","FL",1.3486,1.3486]
["12079","Madison","FL",1.228,1.228]
["12081","Manatee","FL",1.2906,1.2906]
["12083","Marion","FL",1.3303,1.3303]
["12085","Martin","FL",1.1096,1.1096]
["12086","Miami-Dade","FL",1.2906,1.2906]
["12087","Monroe","FL",1.2906,1.2906]
["12089","Nassau","FL",1.349,1.349]
["12091","Okaloosa","FL",1.2469,1.2469]
["12093","Okeechobee","FL",1.2906,1.2906]
["12095","Orange","FL",1.27,1.27]
["12097","Osceola","FL",1.17,1.17]
["12099","Palm Beach","FL",1.2022,1.2022]
["12101","Pasco","FL",1.3124,1.3124]
["12103","Pinellas","FL",1.2906,1.2906]
["12105","Polk","FL",1.332,1.332]
["12107","Putnam","FL",1.2351,1.2351]
["12109","St Johns","FL",1.3066,1.3066]
["12111","St Lucie","FL",1.2022,1.2022]
["12113","Santa Rosa","FL",1.4062,1.4062]
["12115","Sarasota","FL",1.4639,1.4639]
["12117","Seminole","FL",1.346,1.346]
["12119","Sumter","FL",1.3906,1.3906]
["12121","Suwannee","FL",1.4035,1.4035]
["12123","Taylor","FL",1.3532,1.3532]
["12125","Union","FL",1.2548,1.2548]
["12127","Volusia","FL",1.2225,1.2225]
["12129","Wakulla","FL",1.3849,1.3849]
["12131","Walton","FL",1.3449,1.3449]
["12133","Washington","FL",1.3141,1.3141]
["13001","Appling","GA",1.2873,1.2873]
["13003","Atkinson","GA",1.2494,1.2494]
["13005","Bacon","GA",1.4733,1.4733]
["13007","Baker","GA",1.3518,1.3518]
["13009","Baldwin","GA",1.2096,1.2096]
["13011","Banks","GA",1.1511,1.1511]
["13013","Barrow","GA",1.283,1.283]
["13015","Bartow","GA",1.332,1.332]
["13017","Ben Hill","GA",1.2402,1.2402]
["13019","Berrien","GA",1.2705,1.2705]
["13021","Bibb","GA",1.2013,1.2013]
["13023","Bleckley","GA",1.3273,1.3273]
["13025","Brantley","GA",1.3064,1.3064]
["13027","Brooks","GA",1.2854,1.2854]
["13029","Bryan","GA",1.3729,1.3729]
["13031","Bulloch","GA",1.2087,1.2087]
["13033","Burke","GA",1.2744,1.2744]
["13035","Butts","GA",1.4076,1.4076]
["13037","Calhoun","GA",1.1965,1.1965]
["13039","Camden","GA",1.2951,1.2951]
["13043","Candler","GA",1.2279,1.2279]
["13045","Carroll","GA",1.3521,1.3521]
["13047","Catoosa","GA",1.5079,1.5079]
["13049","Charlton","GA",1.3227,1.3227]
["13051","Chatham","GA",1.277,1.277]
["13053","Chattahoochee","GA",1.2935,1.2935]
["13055","Chattooga","GA",1.3202,1.3202]
["13057","Cherokee","GA",1.1472,1.1472]
["13059","Clarke","GA",1.1936,1.1936]
["13061","Clay","GA",1.3256,1.3256]
["13063","Clayton","GA",1.2725,1.2725]
["13065","Clinch","GA",1.221,1.221]
["13067","Cobb","GA",1.1956,1.1956]
["13069","Coffee","GA",1.2095,1.2095]
["13071","Colquitt","GA",1.258,1.258]
["13073","Columbia","GA",1.203,1.203]
["13075","Cook","GA",1.2232,1.2232]
["13077","Coweta","GA",1.1208,1.1208]
["13079","Crawford","GA",1.2319,1.2319]
["13081","Crisp","GA",1.4435,1.4435]
["13083","Dade","GA",1.1937,1.1937]
["13085","Dawson","GA",1.3228,1.3228]
["13087","Decatur","GA",1.3515,1.3515]
["13089","De Kalb","GA",1.2008,1.2008]
["13091","Dodge","GA",1.2411,1.2411]
["13093","Dooly","GA",1.3275,1.3275]
["13095","Dougherty","GA",1.4251,1.4251]
["13097","Douglas","GA",1.1679,1.1679]
["13099","Early","GA",1.2703,1.2703]
["13101","Echols","GA",1.2853,1.2853]
["13103","Effingham","GA",1.362,1.362]
["13105","Elbert","GA",1.2018,1.2018]
["13107","Emanuel","GA",1.1668,1.1668]
["13109","Evans","GA",1.151,1.151]
["13111","Fannin","GA",1.3035,1.3035]
["13113","Fayette","GA",1.2267,1.2267]
["13115","Floyd","GA",1.3228,1.3228]
["13117","Forsyth","GA",1.2712,1.2712]
["13119","Franklin","GA",1.3582,1.3582]
["13121","Fulton","GA",1.2998,1.2998]
["13123","Gilmer","GA",1.2829,1.2829]
["13125","Glascock","GA",1.3257,1.3257]
["13127","Glynn","GA",1.2351,1.2351]
["13129","Gordon","GA",1.2913,1.2913]
["13131","Grady","GA",1.3453,1.3453]
["13133","Greene","GA",1.2022,1.2022]
["13135","Gwinnett","GA",1.2659,1.2659]
["13137","Habersham","GA",1.2828,1.2828]
["13139","Hall","GA",1.1789,1.1789]
["13141","Hancock","GA",1.3288,1.3288]
["13143","Haralson","GA",1.2483,1.2483]
["13145","Harris","GA",1.1728,1.1728]
["13147","Hart","GA",1.3319,1.3319]
["13149","Heard","GA",1.1914,1.1914]
["13151","Henry","GA",1.26,1.26]
["13153","Houston","GA",1.3353,1.3353]
["13155","Irwin","GA",1.3262,1.3262]
["13157","Jackson","GA",1.3418,1.3418]
["13159","Jasper","GA",1.2802,1.2802]
["13161","Jeff Davis","GA",1.4432,1.4432]
["13163","Jefferson","GA",1.3577,1.3577]
["13165","Jenkins","GA",1.2538,1.2538]
["13167","Johnson","GA",1.27,1.27]
["13169","Jones","GA",1.2421,1.2421]
["13171","Lamar","GA",1.4036,1.4036]
["13173","Lanier","GA",1.2363,1.2363]
["13175","Laurens","GA",1.2418,1.2418]
["13177","Lee","GA",1.3399,1.3399]
["13179","Liberty","GA",1.234,1.234]
["13181","Lincoln","GA",1.2661,1.2661]
["13183","Long","GA",1.3011,1.3011]
["13185","Lowndes","GA",1.2532,1.2532]
["13187","Lumpkin","GA",1.3697,1.3697]
["13189","McDuffie","GA",1.1598,1.1598]
["13191","McIntosh","GA",1.2297,1.2297]
["13193","Macon","GA",1.3834,1.3834]
["13195","Madison","GA",1.1474,1.1474]
["13197","Marion","GA",1.2831,1.2831]
["13199","Meriwether","GA",1.2592,1.2592]
["13201","Miller","GA",1.1698,1.1698]
["13205","Mitchell","GA",1.1711,1.1711]
["13207","Monroe","GA",1.3803,1.3803]
["13209","Montgomery","GA",1.2845,1.2845]
["13211","Morgan","GA",1.1919,1.1919]
["13213","Murray","GA",1.3962,1.3962]
["13215","Muscogee","GA",1.3001,1.3001]
["13217","Newton","GA",1.2738,1.2738]
["13219","Oconee","GA",1.2914,1.2914]
["13221","Oglethorpe","GA",1.2638,1.2638]
["13223","Paulding","GA",1.3795,1.3795]
["13225","Peach","GA",1.017,1.017]
["13227","Pickens","GA",1.1532,1.1532]
["13229","Pierce","GA",1.2521,1.2521]
["13231","Pike","GA",1.3095,1.3095]
["13233","Polk","GA",1.3376,1.3376]
["13235","Pulaski","GA",1.3289,1.3289]
["13237","Putnam","GA",1.2806,1.2806]
["13239","Quitman","GA",1.4292,1.4292]
["13241","Rabun","GA",1.3223,1.3223]
["13243","Randolph","GA",1.2788,1.2788]
["13245","Richmond","GA",1.1827,1.1827]
["13247","Rockdale","GA",1.1838,1.1838]
["13249","Schley","GA",1.3262,1.3262]
["13251","Screven","GA",1.2488,1.2488]
["13253","Seminole","GA",1.3811,1.3811]
["13255","Spalding","GA",1.1605,1.1605]
["13257","Stephens","GA",1.328,1.328]
["13259","Stewart","GA",1.3236,1.3236]
["13261","Sumter","GA",1.236,1.236]
["13263","Talbot","GA",1.2425,1.2425]
["13265","Taliaferro","GA",1.2724,1.2724]
["13267","Tattnall","GA",1.1826,1.1826]
["13269","Taylor","GA",1.3003,1.3003]
["13271","Telfair","GA",1.275,1.275]
["13273","Terrell","GA",1.2,1.2]
["13275","Thomas","GA",1.2791,1.2791]
["13277","Tift","GA",1.1632,1.1632]
["13279","Toombs","GA",1.2148,1.2148]
["13281","Towns","GA",1.1133,1.1133]
["13283","Treutlen","GA",1.3232,1.3232]
["13285","Troup","GA",1.2065,1.2065]
["13287","Turner","GA",1.3223,1.3223]
["13289","Twiggs","GA",1.3579,1.3579]
["13291","Union","GA",1.3441,1.3441]
["13293","Upson","GA",1.2777,1.2777]
["13295","Walker","GA",1.1271,1.1271]
["13297","Walton","GA",1.1206,1.1206]
["13299","Ware","GA",1.2714,1.2714]
["13301","Warren","GA",1.2123,1.2123]
["13303","Washington","GA",1.3482,1.3482]
["13305","Wayne","GA",1.2837,1.2837]
["13307","Webster","GA",1.3181,1.3181]
["13309","Wheeler","GA",1.3081,1.3081]
["13311","White","GA",1.3089,1.3089]
["13313","Whitfield","GA",1.3415,1.3415]
["13315","Wilcox","GA",1.346,1.346]
["13317","Wilkes","GA",1.2931,1.2931]
["13319","Wilkinson","GA",1.3097,1.3097]
["13321","Worth","GA",1.2668,1.2668]
["15001","Hawaii","HI",1.0276,1.0276]
["15003","Honolulu","HI",1.0276,1.0276]
["15005","Kalawao","HI",1.0276,1.0276]
["15007","Kauai","HI",1.0276,1.0276]
["15009","Maui","HI",1.0276,1.0276]
["16001","Ada","ID",1.017,1.017]
["16003","Adams","ID",1.0276,1.0276]
["16005","Bannock","ID",1.017,1.017]
["16007","Bear Lake","ID",1.0276,1.0276]
["16009","Benewah","ID",1.017,1.017]
["16011","Bingham","ID",1.0276,1.0276]
["16013","Blaine","ID",1.017,1.017]
["16015","Boise","ID",1.0276,1.0276]
["16017","Bonner","ID",1.0276,1.0276]
["16019","Bonneville","ID",1.0276,1.0276]
["16021","Boundary","ID",1.017,1.017]
["16023","Butte","ID",1.017,1.017]
["16025","Camas","ID",1.0276,1.0276]
["16027","Canyon","ID",1.0276,1.0276]
["16029","Caribou","ID",1.017,1.017]
["16031","Cassia","ID",1.017,1.017]
["16033","Clark","ID",1.017,1.017]
["16035","Clearwater","ID",1.017,1.017]
["16037","Custer","ID",1.0174,1.0174]
["16039","Elmore","ID",1.017,1.017]
["16041","Franklin","ID",1.017,1.017]
["16043","Fremont","ID",1.0276,1.0276]
["16045","Gem","ID",1.017,1.017]
["16047","Gooding","ID",1.0276,1.0276]
["16049","Idaho","ID",1.017,1.017]
["16051","Jefferson","ID",1.0276,1.0276]
["16053","Jerome","ID",1.0276,1.0276]
["16055","Kootenai","ID",1.017,1.017]
["16057","Latah","ID",1.017,1.017]
["16059","Lemhi","ID",1.0276,1.0276]
["16061","Lewis","ID",1.0276,1.0276]
["16063","Lincoln","ID",1.0276,1.0276]
["16065","Madison","ID",1.0276,1.0276]
["16067","Minidoka","ID",1.0276,1.0276]
["16069","Nez Perce","ID",1.0276,1.0276]
["16071","Oneida","ID",1.0276,1.0276]
["16073","Owyhee","ID",1.0276,1.0276]
["16075","Payette","ID",1.0276,1.0276]
["16077","Power","ID",1.017,1.017]
["16079","Shoshone","ID",1.017,1.017]
["16081","Teton","ID",1.0276,1.0276]
["16083","Twin Falls","ID",1.017,1.017]
["16085","Valley","ID",1.017,1.017]
["16087","Washington","ID",1.0276,1.0276]
["17001","Adams","IL",1.3504,1.3504]
["17003","Alexander","IL",1.4811,1.4811]
["17005","Bond","IL",1.3694,1.3694]
["17007","Boone","IL",1.3859,1.3859]
["17009","Brown","IL",1.3343,1.3343]
["17011","Bureau","IL",1.3092,1.3092]
["17013","Calhoun","IL",1.4339,1.4339]
["17015","Carroll","IL",1.3591,1.3591]
["17017","Cass","IL",1.4114,1.4114]
["17019","Champaign","IL",1.1998,1.1998]
["17021","Christian","IL",1.3381,1.3381]
["17023","Clark","IL",1.3397,1.3397]
["17025","Clay","IL",1.4447,1.4447]
["17027","Clinton","IL",1.3683,1.3683]
["17029","Coles","IL",1.3611,1.3611]
["17031","Cook","IL",1.3219,1.3219]
["17033","Crawford","IL",1.4004,1.4004]
["17035","Cumberland","IL",1.3566,1.3566]
["17037","De Kalb","IL",1.3883,1.3883]
["17039","Dewitt","IL",1.1867,1.1867]
["17041","Douglas","IL",1.3277,1.3277]
["17043","Du Page","IL",1.3279,1.3279]
["17045","Edgar","IL",1.1504,1.1504]
["17047","Edwards","IL",1.3431,1.3431]
["17049","Effingham","IL",1.4486,1.4486]
["17051","Fayette","IL",1.4677,1.4677]
["17053","Ford","IL",1.4389,1.4389]
["17055","Franklin","IL",1.418,1.418]
["17057","Fulton","IL",1.2981,1.2981]
["17059","Gallatin","IL",1.3714,1.3714]
["17061","Greene","IL",1.4117,1.4117]
["17063","Grundy","IL",1.3227,1.3227]
["17065","Hamilton","IL",1.4232,1.4232]
["17067","Hancock","IL",1.3747,1.3747]
["17069","Hardin","IL",1.4499,1.4499]
["17071","Henderson","IL",1.332,1.332]
["17073","Henry","IL",1.3253,1.3253]
["17075","Iroquois","IL",1.2516,1.2516]
["17077","Jackson","IL",1.4413,1.4413]
["17079","Jasper","IL",1.3918,1.3918]
["17081","Jefferson","IL",1.3982,1.3982]
["17083","Jersey","IL",1.3451,1.3451]
["17085","Jo Daviess","IL",1.2945,1.2945]
["17087","Johnson","IL",1.4456,1.4456]
["17089","Kane","IL",1.3364,1.3364]
["17091","Kankakee","IL",1.3222,1.3222]
["17093","Kendall","IL",1.3956,1.3956]
["17095","Knox","IL",1.3365,1.3365]
["17097","Lake","IL",1.3873,1.3873]
["17099","La Salle","IL",1.2261,1.2261]
["17101","Lawrence","IL",1.3174,1.3174]
["17103","Lee","IL",1.3069,1.3069]
["17105","Livingston","IL",1.2574,1.2574]
["17107","Logan","IL",1.2868,1.2868]
["17109","McDonough","IL",1.3255,1.3255]
["17111","McHenry","IL",1.3986,1.3986]
["17113","Mclean","IL",1.2806,1.2806]
["17115","Macon","IL",1.1375,1.1375]
["17117","Macoupin","IL",1.3019,1.3019]
["17119","Madison","IL",1.2916,1.2916]
["17121","Marion","IL",1.4358,1.4358]
["17123","Marshall","IL",1.3681,1.3681]
["17125","Mason","IL",1.4318,1.4318]
["17127","Massac","IL",1.4168,1.4168]
["17129","Menard","IL",1.2526,1.2526]
["17131","Mercer","IL",1.3287,1.3287]
["17133","Monroe","IL",1.406,1.406]
["17135","Montgomery","IL",1.3175,1.3175]
["17137","Morgan","IL",1.2829,1.2829]
["17139","Moultrie","IL",1.2542,1.2542]
["17141","Ogle","IL",1.3684,1.3684]
["17143","Peoria","IL",1.3459,1.3459]
["17145","Perry","IL",1.4477,1.4477]
["17147","Piatt","IL",1.3067,1.3067]
["17149","Pike","IL",1.3861,1.3861]
["17151","Pope","IL",1.4156,1.4156]
["17153","Pulaski","IL",1.4372,1.4372]
["17155","Putnam","IL",1.3958,1.3958]
["17157","Randolph","IL",1.3909,1.3909]
["17159","Richland","IL",1.4436,1.4436]
["17161","Rock Island","IL",1.2932,1.2932]
["17163","St Clair","IL",1.3866,1.3866]
["17165","Saline","IL",1.3402,1.3402]
["17167","Sangamon","IL",1.2696,1.2696]
["17169","Schuyler","IL",1.42,1.42]
["17171","Scott","IL",1.3909,1.3909]
["17173","Shelby","IL",1.3631,1.3631]
["17175","Stark","IL",1.3526,1.3526]
["17177","Stephenson","IL",1.2757,1.2757]
["17179","Tazewell","IL",1.3167,1.3167]
["17181","Union","IL",1.4035,1.4035]
["17183","Vermilion","IL",1.3397,1.3397]
["17185","Wabash","IL",1.4252,1.4252]
["17187","Warren","IL",1.3975,1.3975]
["17189","Washington","IL",1.427,1.427]
["17191","Wayne","IL",1.4387,1.4387]
["17193","White","IL",1.4473,1.4473]
["17195","Whiteside","IL",1.3241,1.3241]
["17197","Will","IL",1.3215,1.3215]
["17199","Williamson","IL",1.3582,1.3582]
["17201","Winnebago","IL",1.3105,1.3105]
["17203","Woodford","IL",1.4022,1.4022]
["18001","Adams","IN",1.3635,1.3635]
["18003","Allen","IN",1.2598,1.2598]
["18005","Bartholomew","IN",1.3541,1.3541]
["18007","Benton","IN",1.26,1.26]
["18009","Blackford","IN",1.4386,1.4386]
["18011","Boone","IN",1.2964,1.2964]
["18013","Brown","IN",1.3995,1.3995]
["18015","Carroll","IN",1.2679,1.2679]
["18017","Cass","IN",1.3241,1.3241]
["18019","Clark","IN",1.3006,1.3006]
["18021","Clay","IN",1.3364,1.3364]
["18023","Clinton","IN",1.3207,1.3207]
["18025","Crawford","IN",1.33,1.33]
["18027","Daviess","IN",1.3963,1.3963]
["18029","Dearborn","IN",1.4113,1.4113]
["18031","Decatur","IN",1.3781,1.3781]
["18033","De Kalb","IN",1.3006,1.3006]
["18035","Delaware","IN",1.381,1.381]
["18037","Dubois","IN",1.4426,1.4426]
["18039","Elkhart","IN",1.3297,1.3297]
["18041","Fayette","IN",1.2022,1.2022]
["18043","Floyd","IN",1.4262,1.4262]
["18045","Fountain","IN",1.3208,1.3208]
["18047","Franklin","IN",1.3527,1.3527]
["18049","Fulton","IN",1.2054,1.2054]
["18051","Gibson","IN",1.172,1.172]
["18053","Grant","IN",1.3412,1.3412]
["18055","Greene","IN",1.3816,1.3816]
["18057","Hamilton","IN",1.3285,1.3285]
["18059","Hancock","IN",1.4298,1.4298]
["18061","Harrison","IN",1.4184,1.4184]
["18063","Hendricks","IN",1.3258,1.3258]
["18065","Henry","IN",1.3207,1.3207]
["18067","Howard","IN",1.3217,1.3217]
["18069","Huntington","IN",1.2773,1.2773]
["18071","Jackson","IN",1.3929,1.3929]
["18073","Jasper","IN",1.4212,1.4212]
["18075","Jay","IN",1.4726,1.4726]
["18077","Jefferson","IN",1.3207,1.3207]
["18079","Jennings","IN",1.2309,1.2309]
["18081","Johnson","IN",1.2369,1.2369]
["18083","Knox","IN",1.4009,1.4009]
["18085","Kosciusko","IN",1.2839,1.2839]
["18087","Lagrange","IN",1.2706,1.2706]
["18089","Lake","IN",1.3778,1.3778]
["18091","La Porte","IN",1.2928,1.2928]
["18093","Lawrence","IN",1.3939,1.3939]
["18095","Madison","IN",1.3656,1.3656]
["18097","Marion","IN",1.4042,1.4042]
["18099","Marshall","IN",1.2641,1.2641]
["18101","Martin","IN",1.3682,1.3682]
["18103","Miami","IN",1.2342,1.2342]
["18105","Monroe","IN",1.3838,1.3838]
["18107","Montgomery","IN",1.222,1.222]
["18109","Morgan","IN",1.1834,1.1834]
["18111","Newton","IN",1.4028,1.4028]
["18113","Noble","IN",1.4621,1.4621]
["18115","Ohio","IN",1.3395,1.3395]
["18117","Orange","IN",1.4265,1.4265]
["18119","Owen","IN",1.3812,1.3812]
["18121","Parke","IN",1.3957,1.3957]
["18123","Perry","IN",1.4398,1.4398]
["18125","Pike","IN",1.4157,1.4157]
["18127","Porter","IN",1.3923,1.3923]
["18129","Posey","IN",1.4951,1.4951]
["18131","Pulaski","IN",1.2585,1.2585]
["18133","Putnam","IN",1.4301,1.4301]
["18135","Randolph","IN",1.3009,1.3009]
["18137","Ripley","IN",1.4136,1.4136]
["18139","Rush","IN",1.3207,1.3207]
["18141","St Joseph","IN",1.269,1.269]
["18143","Scott","IN",1.3673,1.3673]
["18145","Shelby","IN",1.3207,1.3207]
["18147","Spencer","IN",1.4898,1.4898]
["18149","Starke","IN",1.3019,1.3019]
["18151","Steuben","IN",1.4338,1.4338]
["18153","Sullivan","IN",1.3921,1.3921]
["18155","Switzerland","IN",1.4133,1.4133]
["18157","Tippecanoe","IN",1.3102,1.3102]
["18159","Tipton","IN",1.3006,1.3006]
["18161","Union","IN",1.3006,1.3006]
["18163","Vanderburgh","IN",1.3713,1.3713]
["18165","Vermillion","IN",1.4239,1.4239]
["18167","Vigo","IN",1.4029,1.4029]
["18169","Wabash","IN",1.3006,1.3006]
["18171","Warren","IN",1.3006,1.3006]
["18173","Warrick","IN",1.3006,1.3006]
["18175","Washington","IN",1.4819,1.4819]
["18177","Wayne","IN",1.3006,1.3006]
["18179","Wells","IN",1.4276,1.4276]
["18181","White","IN",1.3006,1.3006]
["18183","Whitley","IN",1.3344,1.3344]
["19001","Adair","IA",1.3268,1.3268]
["19003","Adams","IA",1.293,1.293]
["19005","Allamakee","IA",1.3329,1.3329]
["19007","Appanoose","IA",1.3541,1.3541]
["19009","Audubon","IA",1.234,1.234]
["19011","Benton","IA",1.351,1.351]
["19013","Black Hawk","IA",1.314,1.314]
["19015","Boone","IA",1.3897,1.3897]
["19017","Bremer","IA",1.308,1.308]
["19019","Buchanan","IA",1.334,1.334]
["19021","Buena Vista","IA",1.3686,1.3686]
["19023","Butler","IA",1.3017,1.3017]
["19025","Calhoun","IA",1.0253,1.0253]
["19027","Carroll","IA",1.0572,1.0572]
["19029","Cass","IA",1.2947,1.2947]
["19031","Cedar","IA",1.3577,1.3577]
["19033","Cerro Gordo","IA",1.3595,1.3595]
["19035","Cherokee","IA",1.3646,1.3646]
["19037","Chickasaw","IA",1.356,1.356]
["19039","Clarke","IA",1.3355,1.3355]
["19041","Clay","IA",1.3013,1.3013]
["19043","Clayton","IA",1.3505,1.3505]
["19045","Clinton","IA",1.283,1.283]
["19047","Crawford","IA",1.3426,1.3426]
["19049","Dallas","IA",1.3566,1.3566]
["19051","Davis","IA",1.3517,1.3517]
["19053","Decatur","IA",1.3116,1.3116]
["19055","Delaware","IA",1.3598,1.3598]
["19057","Des Moines","IA",1.3502,1.3502]
["19059","Dickinson","IA",1.3568,1.3568]
["19061","Dubuque","IA",1.3891,1.3891]
["19063","Emmet","IA",1.2994,1.2994]
["19065","Fayette","IA",1.3428,1.3428]
["19067","Floyd","IA",1.3708,1.3708]
["19069","Franklin","IA",1.3056,1.3056]
["19071","Fremont","IA",1.3094,1.3094]
["19073","Greene","IA",1.2898,1.2898]
["19075","Grundy","IA",1.1432,1.1432]
["19077","Guthrie","IA",1.3663,1.3663]
["19079","Hamilton","IA",1.378,1.378]
["19081","Hancock","IA",1.2838,1.2838]
["19083","Hardin","IA",1.3575,1.3575]
["19085","Harrison","IA",1.3123,1.3123]
["19087","Henry","IA",1.387,1.387]
["19089","Howard","IA",1.3685,1.3685]
["19091","Humboldt","IA",1.3449,1.3449]
["19093","Ida","IA",1.003,1.003]
["19095","Iowa","IA",1.302,1.302]
["19097","Jackson","IA",1.3244,1.3244]
["19099","Jasper","IA",1.3387,1.3387]
["19101","Jefferson","IA",1.3653,1.3653]
["19103","Johnson","IA",1.3638,1.3638]
["19105","Jones","IA",1.3222,1.3222]
["19107","Keokuk","IA",1.3145,1.3145]
["19109","Kossuth","IA",1.284,1.284]
["19111","Lee","IA",1.393,1.393]
["19113","Linn","IA",1.3599,1.3599]
["19115","Louisa","IA",1.2419,1.2419]
["19117","Lucas","IA",1.3326,1.3326]
["19119","Lyon","IA",1.3481,1.3481]
["19121","Madison","IA",1.3465,1.3465]
["19123","Mahaska","IA",1.3217,1.3217]
["19125","Marion","IA",1.3752,1.3752]
["19127","Marshall","IA",1.3232,1.3232]
["19129","Mills","IA",1.3006,1.3006]
["19131","Mitchell","IA",1.356,1.356]
["19133","Monona","IA",1.3155,1.3155]
["19135","Monroe","IA",1.3552,1.3552]
["19137","Montgomery","IA",1.2999,1.2999]
["19139","Muscatine","IA",1.3196,1.3196]
["19141","Obrien","IA",1.1146,1.1146]
["19143","Osceola","IA",1.1481,1.1481]
["19145","Page","IA",1.3017,1.3017]
["19147","Palo Alto","IA",1.2634,1.2634]
["19149","Plymouth","IA",1.3219,1.3219]
["19151","Pocahontas","IA",1.1195,1.1195]
["19153","Polk","IA",1.2543,1.2543]
["19155","Pottawattamie","IA",1.362,1.362]
["19157","Poweshiek","IA",1.3729,1.3729]
["19159","Ringgold","IA",1.2978,1.2978]
["19161","Sac","IA",1.2911,1.2911]
["19163","Scott","IA",1.3347,1.3347]
["19165","Shelby","IA",1.282,1.282]
["19167","Sioux","IA",1.0558,1.0558]
["19169","Story","IA",1.3845,1.3845]
["19171","Tama","IA",1.3204,1.3204]
["19173","Taylor","IA",1.3125,1.3125]
["19175","Union","IA",1.3115,1.3115]
["19177","Van Buren","IA",1.3655,1.3655]
["19179","Wapello","IA",1.3762,1.3762]
["19181","Warren","IA",1.3365,1.3365]
["19183","Washington","IA",1.3092,1.3092]
["19185","Wayne","IA",1.3425,1.3425]
["19187","Webster","IA",1.39,1.39]
["19189","Winnebago","IA",1.3447,1.3447]
["19191","Winneshiek","IA",1.3516,1.3516]
["19193","Woodbury","IA",1.3681,1.3681]
["19195","Worth","IA",1.3414,1.3414]
["19197","Wright","IA",1.3537,1.3537]
["20001","Allen","KS",1.2458,1.2458]
["20003","Anderson","KS",1.2457,1.2457]
["20005","Atchison","KS",1.2565,1.2565]
["20007","Barber","KS",1.1584,1.1584]
["20009","Barton","KS",1.1567,1.1567]
["20011","Bourbon","KS",1.2407,1.2407]
["20013","Brown","KS",1.2288,1.2288]
["20015","Butler","KS",1.2124,1.2124]
["20017","Chase","KS",1.3349,1.3349]
["20019","Chautauqua","KS",1.4163,1.4163]
["20021","Cherokee","KS",1.2321,1.2321]
["20023","Cheyenne","KS",1.3006,1.3006]
["20025","Clark","KS",1.3006,1.3006]
["20027","Clay","KS",1.2389,1.2389]
["20029","Cloud","KS",1.348,1.348]
["20031","Coffey","KS",1.304,1.304]
["20033","Comanche","KS",1.3006,1.3006]
["20035","Cowley","KS",1.2249,1.2249]
["20037","Crawford","KS",1.2203,1.2203]
["20039","Decatur","KS",1.3006,1.3006]
["20041","Dickinson","KS",1.2343,1.2343]
["20043","Doniphan","KS",1.1307,1.1307]
["20045","Douglas","KS",1.2051,1.2051]
["20047","Edwards","KS",1.3006,1.3006]
["20049","Elk","KS",1.4289,1.4289]
["20051","Ellis","KS",1.2702,1.2702]
["20053","Ellsworth","KS",1.3006,1.3006]
["20055","Finney","KS",1.139,1.139]
["20057","Ford","KS",1.1059,1.1059]
["20059","Franklin","KS",1.2704,1.2704]
["20061","Geary","KS",1.2454,1.2454]
["20063","Gove","KS",1.3006,1.3006]
["20065","Graham","KS",1.3006,1.3006]
["20067","Grant","KS",1.3006,1.3006]
["20069","Gray","KS",0.9962,0.9962]
["20071","Greeley","KS",1.3006,1.3006]
["20073","Greenwood","KS",1.2636,1.2636]
["20075","Hamilton","KS",1.272,1.272]
["20077","Harper","KS",1.2078,1.2078]
["20079","Harvey","KS",1.1567,1.1567]
["20081","Haskell","KS",1.3006,1.3006]
["20083","Hodgeman","KS",1.3006,1.3006]
["20085","Jackson","KS",1.3367,1.3367]
["20087","Jefferson","KS",1.2935,1.2935]
["20089","Jewell","KS",1.3041,1.3041]
["20091","Johnson","KS",1.254,1.254]
["20093","Kearny","KS",1.3006,1.3006]
["20095","Kingman","KS",1.2136,1.2136]
["20097","Kiowa","KS",0.924,0.924]
["20099","Labette","KS",1.229,1.229]
["20101","Lane","KS",1.3006,1.3006]
["20103","Leavenworth","KS",1.3553,1.3553]
["20105","Lincoln","KS",1.3006,1.3006]
["20107","Linn","KS",1.2263,1.2263]
["20109","Logan","KS",1.3006,1.3006]
["20111","Lyon","KS",1.2185,1.2185]
["20113","McPherson","KS",1.2027,1.2027]
["20115","Marion","KS",1.2045,1.2045]
["20117","Marshall","KS",1.2335,1.2335]
["20119","Meade","KS",1.24,1.24]
["20121","Miami","KS",1.3527,1.3527]
["20123","Mitchell","KS",1.1634,1.1634]
["20125","Montgomery","KS",1.2283,1.2283]
["20127","Morris","KS",1.3006,1.3006]
["20129","Morton","KS",1.3006,1.3006]
["20131","Nemaha","KS",1.2022,1.2022]
["20133","Neosho","KS",1.3118,1.3118]
["20135","Ness","KS",0.9961,0.9961]
["20137","Norton","KS",1.3006,1.3006]
["20139","Osage","KS",1.2022,1.2022]
["20141","Osborne","KS",1.1634,1.1634]
["20143","Ottawa","KS",1.1634,1.1634]
["20145","Pawnee","KS",1.2077,1.2077]
["20147","Phillips","KS",1.3006,1.3006]
["20149","Pottawatomie","KS",1.239,1.239]
["20151","Pratt","KS",1.2084,1.2084]
["20153","Rawlins","KS",1.3006,1.3006]
["20155","Reno","KS",1.1561,1.1561]
["20157","Republic","KS",1.396,1.396]
["20159","Rice","KS",1.0004,1.0004]
["20161","Riley","KS",1.3564,1.3564]
["20163","Rooks","KS",1.3006,1.3006]
["20165","Rush","KS",1.3006,1.3006]
["20167","Russell","KS",1.2168,1.2168]
["20169","Saline","KS",1.1858,1.1858]
["20171","Scott","KS",1.3006,1.3006]
["20173","Sedgwick","KS",1.1604,1.1604]
["20175","Seward","KS",1.3006,1.3006]
["20177","Shawnee","KS",1.2929,1.2929]
["20179","Sheridan","KS",1.2702,1.2702]
["20181","Sherman","KS",1.2041,1.2041]
["20183","Smith","KS",1.0693,1.0693]
["20185","Stafford","KS",1.3006,1.3006]
["20187","Stanton","KS",1.3006,1.3006]
["20189","Stevens","KS",1.3006,1.3006]
["20191","Sumner","KS",1.1928,1.1928]
["20193","Thomas","KS",1.1634,1.1634]
["20195","Trego","KS",0.924,0.924]
["20197","Wabaunsee","KS",1.3666,1.3666]
["20199","Wallace","KS",1.1768,1.1768]
["20201","Washington","KS",1.3621,1.3621]
["20203","Wichita","KS",1.3006,1.3006]
["20205","Wilson","KS",1.1907,1.1907]
["20207","Woodson","KS",1.24,1.24]
["20209","Wyandotte","KS",1.363,1.363]
["21001","Adair","KY",1.2324,1.2324]
["21003","Allen","KY",1.431,1.431]
["21005","Anderson","KY",1.3762,1.3762]
["21007","Ballard","KY",1.292,1.292]
["21009","Barren","KY",1.2488,1.2488]
["21011","Bath","KY",1.4451,1.4451]
["21013","Bell","KY",1.3363,1.3363]
["21015","Boone","KY",1.2022,1.2022]
["21017","Bourbon","KY",1.2022,1.2022]
["21019","Boyd","KY",1.396,1.396]
["21021","Boyle","KY",1.4245,1.4245]
["21023","Bracken","KY",1.2022,1.2022]
["21025","Breathitt","KY",1.3536,1.3536]
["21027","Breckinridge","KY",1.2683,1.2683]
["21029","Bullitt","KY",1.24,1.24]
["21031","Butler","KY",1.2642,1.2642]
["21033","Caldwell","KY",1.4396,1.4396]
["21035","Calloway","KY",1.4506,1.4506]
["21037","Campbell","KY",1.2906,1.2906]
["21039","Carlisle","KY",1.4008,1.4008]
["21041","Carroll","KY",1.4389,1.4389]
["21043","Carter","KY",1.3425,1.3425]
["21045","Casey","KY",1.4124,1.4124]
["21047","Christian","KY",1.4071,1.4071]
["21049","Clark","KY",1.2022,1.2022]
["21051","Clay","KY",1.4278,1.4278]
["21053","Clinton","KY",1.4499,1.4499]
["21055","Crittenden","KY",1.2614,1.2614]
["21057","Cumberland","KY",1.4191,1.4191]
["21059","Daviess","KY",1.4047,1.4047]
["21061","Edmonson","KY",1.4662,1.4662]
["21063","Elliott","KY",1.3706,1.3706]
["21065","Estill","KY",1.4114,1.4114]
["21067","Fayette","KY",1.2022,1.2022]
["21069","Fleming","KY",1.396,1.396]
["21071","Floyd","KY",1.2768,1.2768]
["21073","Franklin","KY",1.2906,1.2906]
["21075","Fulton","KY",1.148,1.148]
["21077","Gallatin","KY",1.572,1.572]
["21079","Garrard","KY",1.2022,1.2022]
["21081","Grant","KY",1.2139,1.2139]
["21083","Graves","KY",1.4245,1.4245]
["21085","Grayson","KY",1.3332,1.3332]
["21087","Green","KY",1.4303,1.4303]
["21089","Greenup","KY",1.2699,1.2699]
["21091","Hancock","KY",1.3028,1.3028]
["21093","Hardin","KY",1.3716,1.3716]
["21095","Harlan","KY",1.1995,1.1995]
["21097","Harrison","KY",1.2022,1.2022]
["21099","Hart","KY",1.3523,1.3523]
["21101","Henderson","KY",1.2022,1.2022]
["21103","Henry","KY",1.1652,1.1652]
["21105","Hickman","KY",1.275,1.275]
["21107","Hopkins","KY",1.2687,1.2687]
["21109","Jackson","KY",1.4435,1.4435]
["21111","Jefferson","KY",1.348,1.348]
["21113","Jessamine","KY",1.2022,1.2022]
["21115","Johnson","KY",1.3132,1.3132]
["21117","Kenton","KY",1.2887,1.2887]
["21119","Knott","KY",1,1]
["21121","Knox","KY",1.2956,1.2956]
["21123","Larue","KY",1.2022,1.2022]
["21125","Laurel","KY",1.3471,1.3471]
["21127","Lawrence","KY",1.1655,1.1655]
["21129","Lee","KY",1.2719,1.2719]
["21131","Leslie","KY",1.3881,1.3881]
["21133","Letcher","KY",1.1527,1.1527]
["21135","Lewis","KY",1.3631,1.3631]
["21137","Lincoln","KY",1.4977,1.4977]
["21139","Livingston","KY",1.4635,1.4635]
["21141","Logan","KY",1.3638,1.3638]
["21143","Lyon","KY",1.4441,1.4441]
["21145","McCracken","KY",1.4559,1.4559]
["21147","McCreary","KY",1.1872,1.1872]
["21149","Mclean","KY",1.2022,1.2022]
["21151","Madison","KY",1.2022,1.2022]
["21153","Magoffin","KY",1.2179,1.2179]
["21155","Marion","KY",1.339,1.339]
["21157","Marshall","KY",1.4436,1.4436]
["21159","Martin","KY",1.4574,1.4574]
["21161","Mason","KY",1.3752,1.3752]
["21163","Meade","KY",1.4332,1.4332]
["21165","Menifee","KY",1.4204,1.4204]
["21167","Mercer","KY",1.2022,1.2022]
["21169","Metcalfe","KY",1.4086,1.4086]
["21171","Monroe","KY",1.4108,1.4108]
["21173","Montgomery","KY",1.2022,1.2022]
["21175","Morgan","KY",1.3146,1.3146]
["21177","Muhlenberg","KY",1.2516,1.2516]
["21179","Nelson","KY",1.4131,1.4131]
["21181","Nicholas","KY",1.2906,1.2906]
["21183","Ohio","KY",1.3415,1.3415]
["21185","Oldham","KY",1.2022,1.2022]
["21187","Owen","KY",1.5208,1.5208]
["21189","Owsley","KY",1.396,1.396]
["21191","Pendleton","KY",1.017,1.017]
["21193","Perry","KY",1.3437,1.3437]
["21195","Pike","KY",1.2663,1.2663]
["21197","Powell","KY",1.1041,1.1041]
["21199","Pulaski","KY",1.4138,1.4138]
["21201","Robertson","KY",1.2906,1.2906]
["21203","Rockcastle","KY",1.4028,1.4028]
["21205","Rowan","KY",1.4701,1.4701]
["21207","Russell","KY",1.2908,1.2908]
["21209","Scott","KY",1.272,1.272]
["21211","Shelby","KY",1.348,1.348]
["21213","Simpson","KY",1.3838,1.3838]
["21215","Spencer","KY",1.379,1.379]
["21217","Taylor","KY",1.3783,1.3783]
["21219","Todd","KY",1.4557,1.4557]
["21221","Trigg","KY",1.3978,1.3978]
["21223","Trimble","KY",1.2022,1.2022]
["21225","Union","KY",1.2022,1.2022]
["21227","Warren","KY",1.3878,1.3878]
["21229","Washington","KY",1.2022,1.2022]
["21231","Wayne","KY",1.4667,1.4667]
["21233","Webster","KY",1.2022,1.2022]
["21235","Whitley","KY",1.3924,1.3924]
["21237","Wolfe","KY",1.4255,1.4255]
["21239","Woodford","KY",1.2906,1.2906]
["22001","Acadia","LA",1.3303,1.3303]
["22003","Allen","LA",1.3007,1.3007]
["22005","Ascension","LA",1.1549,1.1549]
["22007","Assumption","LA",1.1574,1.1574]
["22009","Avoyelles","LA",1.388,1.388]
["22011","Beauregard","LA",1.2455,1.2455]
["22013","Bienville","LA",1.3097,1.3097]
["22015","Bossier","LA",1.3892,1.3892]
["22017","Caddo","LA",1.3066,1.3066]
["22019","Calcasieu","LA",1.3386,1.3386]
["22021","Caldwell","LA",1.3857,1.3857]
["22023","Cameron","LA",1.2906,1.2906]
["22025","Catahoula","LA",1.2007,1.2007]
["22027","Claiborne","LA",1.2679,1.2679]
["22029","Concordia","LA",1.2049,1.2049]
["22031","De Soto","LA",1.3541,1.3541]
["22033","East Baton Rouge","LA",1.2326,1.2326]
["22035","East Carroll","LA",1.1294,1.1294]
["22037","East Feliciana","LA",1.2788,1.2788]
["22039","Evangeline","LA",1.2954,1.2954]
["22041","Franklin","LA",1.2808,1.2808]
["22043","Grant","LA",1.2536,1.2536]
["22045","Iberia","LA",1.2906,1.2906]
["22047","Iberville","LA",1.2044,1.2044]
["22049","Jackson","LA",1.3833,1.3833]
["22051","Jefferson","LA",1.2906,1.2906]
["22053","Jefferson Davis","LA",1.1493,1.1493]
["22055","Lafayette","LA",1.2022,1.2022]
["22057","Lafourche","LA",1.2839,1.2839]
["22059","LaSalle","LA",1.3612,1.3612]
["22061","Lincoln","LA",1.2289,1.2289]
["22063","Livingston","LA",1.2357,1.2357]
["22065","Madison","LA",1.2674,1.2674]
["22067","Morehouse","LA",1.3002,1.3002]
["22069","Natchitoches","LA",1.3617,1.3617]
["22071","Orleans","LA",1.2839,1.2839]
["22073","Ouachita","LA",1.4382,1.4382]
["22075","Plaquemines","LA",1.2839,1.2839]
["22077","Pointe Coupee","LA",1.3527,1.3527]
["22079","Rapides","LA",1.4025,1.4025]
["22081","Red River","LA",1.2039,1.2039]
["22083","Richland","LA",1.3998,1.3998]
["22085","Sabine","LA",1.2535,1.2535]
["22087","St Bernard","LA",1.2839,1.2839]
["22089","St Charles","LA",1.2906,1.2906]
["22091","St Helena","LA",1.2523,1.2523]
["22093","St James","LA",1.1,1.1]
["22095","St John The Baptist","LA",1.2906,1.2906]
["22097","St Landry","LA",1.2967,1.2967]
["22099","St Martin","LA",1.1704,1.1704]
["22101","St Mary","LA",1.2906,1.2906]
["22103","St Tammany","LA",1.277,1.277]
["22105","Tangipahoa","LA",1.2931,1.2931]
["22107","Tensas","LA",1.1838,1.1838]
["22109","Terrebonne","LA",1.148,1.148]
["22111","Union","LA",1.2889,1.2889]
["22113","Vermilion","LA",1.2906,1.2906]
["22115","Vernon","LA",1.3117,1.3117]
["22117","Washington","LA",1.2358,1.2358]
["22119","Webster","LA",1.3543,1.3543]
["22121","West Baton Rouge","LA",1.2783,1.2783]
["22123","West Carroll","LA",1.1979,1.1979]
["22125","West Feliciana","LA",1.1871,1.1871]
["22127","Winn","LA",1.3259,1.3259]
["23001","Androscoggin","ME",1.1645,1.1645]
["23003","Aroostook","ME",1.1883,1.1883]
["23005","Cumberland","ME",1.2008,1.2008]
["23007","Franklin","ME",1.2102,1.2102]
["23009","Hancock","ME",1.1921,1.1921]
["23011","Kennebec","ME",1.1913,1.1913]
["23013","Knox","ME",1.164,1.164]
["23015","Lincoln","ME",1.1904,1.1904]
["23017","Oxford","ME",1.1973,1.1973]
["23019","Penobscot","ME",1.1888,1.1888]
["23021","Piscataquis","ME",1.1972,1.1972]
["23023","Sagadahoc","ME",1.1954,1.1954]
["23025","Somerset","ME",1.1898,1.1898]
["23027","Waldo","ME",1.1573,1.1573]
["23029","Washington","ME",1.1979,1.1979]
["23031","York","ME",1.1835,1.1835]
["24001","Allegany","MD",1.2236,1.2236]
["24003","Anne Arundel","MD",1.2104,1.2104]
["24005","Baltimore","MD",1.1944,1.1944]
["24009","Calvert","MD",1.1559,1.1559]
["24011","Caroline","MD",1.2051,1.2051]
["24013","Carroll","MD",1.2629,1.2629]
["24015","Cecil","MD",1.1445,1.1445]
["24017","Charles","MD",1.2473,1.2473]
["24019","Dorchester","MD",1.2114,1.2114]
["24021","Frederick","MD",1.322,1.322]
["24023","Garrett","MD",1.2465,1.2465]
["24025","Harford","MD",1.2047,1.2047]
["24027","Howard","MD",1.1838,1.1838]
["24029","Kent","MD",1.2738,1.2738]
["24031","Montgomery","MD",1.1566,1.1566]
["24033","Prince Georges","MD",1.2575,1.2575]
["24035","Queen Annes","MD",1.2818,1.2818]
["24037","St Marys","MD",1.2208,1.2208]
["24039","Somerset","MD",1.1805,1.1805]
["24041","Talbot","MD",1.1933,1.1933]
["24043","Washington","MD",1.3965,1.3965]
["24045","Wicomico","MD",1.2093,1.2093]
["24047","Worcester","MD",1.1931,1.1931]
["24510","Baltimore City","MD",1.2906,1.2906]
["25001","Barnstable","MA",1.2934,1.2934]
["25003","Berkshire","MA",1.275,1.275]
["25005","Bristol","MA",1.0182,1.0182]
["25007","Dukes","MA",1.1798,1.1798]
["25009","Essex","MA",1.0173,1.0173]
["25011","Franklin","MA",1.2723,1.2723]
["25013","Hampden","MA",1.2338,1.2338]
["25015","Hampshire","MA",1.193,1.193]
["25017","Middlesex","MA",1.0944,1.0944]
["25019","Nantucket","MA",1.2934,1.2934]
["25021","Norfolk","MA",0.8643,0.8643]
["25023","Plymouth","MA",0.8891,0.8891]
["25025","Suffolk","MA",1.2934,1.2934]
["25027","Worcester","MA",1.1889,1.1889]
["26001","Alcona","MI",1.1725,1.1725]
["26003","Alger","MI",1.386,1.386]
["26005","Allegan","MI",1.3153,1.3153]
["26007","Alpena","MI",1.1518,1.1518]
["26009","Antrim","MI",1.2376,1.2376]
["26011","Arenac","MI",1.2737,1.2737]
["26013","Baraga","MI",1.3875,1.3875]
["26015","Barry","MI",1.3626,1.3626]
["26017","Bay","MI",1.3006,1.3006]
["26019","Benzie","MI",1.3053,1.3053]
["26021","Berrien","MI",1.1641,1.1641]
["26023","Branch","MI",1.3006,1.3006]
["26025","Calhoun","MI",1.4437,1.4437]
["26027","Cass","MI",1.2775,1.2775]
["26029","Charlevoix","MI",1.2746,1.2746]
["26031","Cheboygan","MI",1.2005,1.2005]
["26033","Chippewa","MI",1.2161,1.2161]
["26035","Clare","MI",1.3006,1.3006]
["26037","Clinton","MI",1.2475,1.2475]
["26039","Crawford","MI",1.3006,1.3006]
["26041","Delta","MI",1.2887,1.2887]
["26043","Dickinson","MI",1.2163,1.2163]
["26045","Eaton","MI",1.2488,1.2488]
["26047","Emmet","MI",1.2618,1.2618]
["26049","Genesee","MI",1.2772,1.2772]
["26051","Gladwin","MI",1.3006,1.3006]
["26053","Gogebic","MI",1.4287,1.4287]
["26055","Grand Traverse","MI",1.2844,1.2844]
["26057","Gratiot","MI",1.4148,1.4148]
["26059","Hillsdale","MI",1.0097,1.0097]
["26061","Houghton","MI",1.4249,1.4249]
["26063","Huron","MI",1.4268,1.4268]
["26065","Ingham","MI",1.2858,1.2858]
["26067","Ionia","MI",1.322,1.322]
["26069","Iosco","MI",1.3006,1.3006]
["26071","Iron","MI",1.3938,1.3938]
["26073","Isabella","MI",1.3006,1.3006]
["26075","Jackson","MI",1.2615,1.2615]
["26077","Kalamazoo","MI",1.2869,1.2869]
["26079","Kalkaska","MI",1.2478,1.2478]
["26081","Kent","MI",1.2787,1.2787]
["26083","Keweenaw","MI",1.4005,1.4005]
["26085","Lake","MI",1.3122,1.3122]
["26087","Lapeer","MI",1.2545,1.2545]
["26089","Leelanau","MI",1.3229,1.3229]
["26091","Lenawee","MI",1.273,1.273]
["26093","Livingston","MI",1.3201,1.3201]
["26095","Luce","MI",1.1356,1.1356]
["26097","Mackinac","MI",1.3573,1.3573]
["26099","Macomb","MI",1.3077,1.3077]
["26101","Manistee","MI",1.2601,1.2601]
["26103","Marquette","MI",1.3888,1.3888]
["26105","Mason","MI",1.26,1.26]
["26107","Mecosta","MI",1.3006,1.3006]
["26109","Menominee","MI",1.3871,1.3871]
["26111","Midland","MI",1.3006,1.3006]
["26113","Missaukee","MI",1.3214,1.3214]
["26115","Monroe","MI",1.3006,1.3006]
["26117","Montcalm","MI",1.3506,1.3506]
["26119","Montmorency","MI",1.1527,1.1527]
["26121","Muskegon","MI",1.36,1.36]
["26123","Newaygo","MI",1.3006,1.3006]
["26125","Oakland","MI",1.2613,1.2613]
["26127","Oceana","MI",1.3006,1.3006]
["26129","Ogemaw","MI",1.3006,1.3006]
["26131","Ontonagon","MI",1.4129,1.4129]
["26133","Osceola","MI",1.1781,1.1781]
["26135","Oscoda","MI",1.2354,1.2354]
["26137","Otsego","MI",1.1795,1.1795]
["26139","Ottawa","MI",1.2656,1.2656]
["26141","Presque Isle","MI",1.1611,1.1611]
["26143","Roscommon","MI",1.3006,1.3006]
["26145","Saginaw","MI",1.1845,1.1845]
["26147","St Clair","MI",1.3013,1.3013]
["26149","St Joseph","MI",1.4422,1.4422]
["26151","Sanilac","MI",1.348,1.348]
["26153","Schoolcraft","MI",1.3367,1.3367]
["26155","Shiawassee","MI",1.2291,1.2291]
["26157","Tuscola","MI",1.3006,1.3006]
["26159","Van Buren","MI",1.3006,1.3006]
["26161","Washtenaw","MI",1.301,1.301]
["26163","Wayne","MI",1.3006,1.3006]
["26165","Wexford","MI",1.261,1.261]
["27001","Aitkin","MN",1.1609,1.1609]
["27003","Anoka","MN",1.3513,1.3513]
["27005","Becker","MN",1.2879,1.2879]
["27007","Beltrami","MN",1.1981,1.1981]
["27009","Benton","MN",1.3006,1.3006]
["27011","Big Stone","MN",1.3377,1.3377]
["27013","Blue Earth","MN",1.3006,1.3006]
["27015","Brown","MN",1.3006,1.3006]
["27017","Carlton","MN",1.1705,1.1705]
["27019","Carver","MN",1.2126,1.2126]
["27021","Cass","MN",1.2355,1.2355]
["27023","Chippewa","MN",1.3006,1.3006]
["27025","Chisago","MN",1.3758,1.3758]
["27027","Clay","MN",1.3589,1.3589]
["27029","Clearwater","MN",1.3006,1.3006]
["27031","Cook","MN",1.1943,1.1943]
["27033","Cottonwood","MN",1.3006,1.3006]
["27035","Crow Wing","MN",1.2361,1.2361]
["27037","Dakota","MN",1.2463,1.2463]
["27039","Dodge","MN",1.3212,1.3212]
["27041","Douglas","MN",1.1269,1.1269]
["27043","Faribault","MN",1.2968,1.2968]
["27045","Fillmore","MN",1.2639,1.2639]
["27047","Freeborn","MN",1.2968,1.2968]
["27049","Goodhue","MN",1.2758,1.2758]
["27051","Grant","MN",1.3006,1.3006]
["27053","Hennepin","MN",1.3645,1.3645]
["27055","Houston","MN",1.3006,1.3006]
["27057","Hubbard","MN",1.1242,1.1242]
["27059","Isanti","MN",1.4071,1.4071]
["27061","Itasca","MN",1.1531,1.1531]
["27063","Jackson","MN",1.3006,1.3006]
["27065","Kanabec","MN",1.2997,1.2997]
["27067","Kandiyohi","MN",1.3006,1.3006]
["27069","Kittson","MN",1.3006,1.3006]
["27071","Koochiching","MN",1.1601,1.1601]
["27073","Lac Qui Parle","MN",1.3006,1.3006]
["27075","Lake","MN",1.1528,1.1528]
["27077","Lake of The Woods","MN",1.1937,1.1937]
["27079","Le Sueur","MN",1.3006,1.3006]
["27081","Lincoln","MN",1.349,1.349]
["27083","Lyon","MN",1.3006,1.3006]
["27085","McLeod","MN",1.3911,1.3911]
["27087","Mahnomen","MN",1.184,1.184]
["27089","Marshall","MN",1.3006,1.3006]
["27091","Martin","MN",1.3139,1.3139]
["27093","Meeker","MN",1.3139,1.3139]
["27095","Mille Lacs","MN",1.2127,1.2127]
["27097","Morrison","MN",1.3668,1.3668]
["27099","Mower","MN",1.3006,1.3006]
["27101","Murray","MN",1.3006,1.3006]
["27103","Nicollet","MN",1.327,1.327]
["27105","Nobles","MN",1.3006,1.3006]
["27107","Norman","MN",1.3006,1.3006]
["27109","Olmsted","MN",1.3541,1.3541]
["27111","Otter Tail","MN",1.3587,1.3587]
["27113","Pennington","MN",1.3006,1.3006]
["27115","Pine","MN",1.2712,1.2712]
["27117","Pipestone","MN",1.3006,1.3006]
["27119","Polk","MN",1.3006,1.3006]
["27121","Pope","MN",0.924,0.924]
["27123","Ramsey","MN",1.2909,1.2909]
["27125","Red Lake","MN",1.2351,1.2351]
["27127","Redwood","MN",1.3733,1.3733]
["27129","Renville","MN",1.3006,1.3006]
["27131","Rice","MN",1.2138,1.2138]
["27133","Rock","MN",1.293,1.293]
["27135","Roseau","MN",1.0353,1.0353]
["27137","St Louis","MN",1.0969,1.0969]
["27139","Scott","MN",1.3006,1.3006]
["27141","Sherburne","MN",1.4059,1.4059]
["27143","Sibley","MN",1.2968,1.2968]
["27145","Stearns","MN",1.3953,1.3953]
["27147","Steele","MN",1.3157,1.3157]
["27149","Stevens","MN",1.3006,1.3006]
["27151","Swift","MN",1.3006,1.3006]
["27153","Todd","MN",1.3006,1.3006]
["27155","Traverse","MN",1.3006,1.3006]
["27157","Wabasha","MN",1.3601,1.3601]
["27159","Wadena","MN",1.3419,1.3419]
["27161","Waseca","MN",1.311,1.311]
["27163","Washington","MN",1.4369,1.4369]
["27165","Watonwan","MN",1.3006,1.3006]
["27167","Wilkin","MN",1.3006,1.3006]
["27169","Winona","MN",1.3006,1.3006]
["27171","Wright","MN",1.2588,1.2588]
["27173","Yellow Medicine","MN",1.3006,1.3006]
["28001","Adams","MS",1.2327,1.2327]
["28003","Alcorn","MS",1.2992,1.2992]
["28005","Amite","MS",1.3104,1.3104]
["28007","Attala","MS",1.2829,1.2829]
["28009","Benton","MS",1.3358,1.3358]
["28011","Bolivar","MS",1.2328,1.2328]
["28013","Calhoun","MS",1.2311,1.2311]
["28015","Carroll","MS",1.3198,1.3198]
["28017","Chickasaw","MS",1.3068,1.3068]
["28019","Choctaw","MS",1.2788,1.2788]
["28021","Claiborne","MS",1.3497,1.3497]
["28023","Clarke","MS",1.3509,1.3509]
["28025","Clay","MS",1.3399,1.3399]
["28027","Coahoma","MS",1.2802,1.2802]
["28029","Copiah","MS",1.2921,1.2921]
["28031","Covington","MS",1.2568,1.2568]
["28033","De Soto","MS",1.361,1.361]
["28035","Forrest","MS",1.3445,1.3445]
["28037","Franklin","MS",1.3153,1.3153]
["28039","George","MS",1.2204,1.2204]
["28041","Greene","MS",1.3374,1.3374]
["28043","Grenada","MS",1.3113,1.3113]
["28045","Hancock","MS",1.3085,1.3085]
["28047","Harrison","MS",1.3562,1.3562]
["28049","Hinds","MS",1.3805,1.3805]
["28051","Holmes","MS",1.3441,1.3441]
["28053","Humphreys","MS",1.2022,1.2022]
["28055","Issaquena","MS",1.226,1.226]
["28057","Itawamba","MS",1.258,1.258]
["28059","Jackson","MS",1.293,1.293]
["28061","Jasper","MS",1.2742,1.2742]
["28063","Jefferson","MS",1.2958,1.2958]
["28065","Jefferson Davis","MS",1.2953,1.2953]
["28067","Jones","MS",1.2832,1.2832]
["28069","Kemper","MS",1.226,1.226]
["28071","Lafayette","MS",1.3416,1.3416]
["28073","Lamar","MS",1.2276,1.2276]
["28075","Lauderdale","MS",1.3201,1.3201]
["28077","Lawrence","MS",1.3113,1.3113]
["28079","Leake","MS",1.3131,1.3131]
["28081","Lee","MS",1.3161,1.3161]
["28083","Leflore","MS",1.4029,1.4029]
["28085","Lincoln","MS",1.2874,1.2874]
["28087","Lowndes","MS",1.3279,1.3279]
["28089","Madison","MS",1.3363,1.3363]
["28091","Marion","MS",1.2832,1.2832]
["28093","Marshall","MS",1.2663,1.2663]
["28095","Monroe","MS",1.2228,1.2228]
["28097","Montgomery","MS",1.3432,1.3432]
["28099","Neshoba","MS",1.2888,1.2888]
["28101","Newton","MS",1.3027,1.3027]
["28103","Noxubee","MS",1.3452,1.3452]
["28105","Oktibbeha","MS",1.271,1.271]
["28107","Panola","MS",1.3597,1.3597]
["28109","Pearl River","MS",1.2501,1.2501]
["28111","Perry","MS",1.2746,1.2746]
["28113","Pike","MS",1.2705,1.2705]
["28115","Pontotoc","MS",1.314,1.314]
["28117","Prentiss","MS",1.3651,1.3651]
["28119","Quitman","MS",1.1989,1.1989]
["28121","Rankin","MS",1.3492,1.3492]
["28123","Scott","MS",1.3102,1.3102]
["28125","Sharkey","MS",1.4261,1.4261]
["28127","Simpson","MS",1.3403,1.3403]
["28129","Smith","MS",1.3024,1.3024]
["28131","Stone","MS",1.3094,1.3094]
["28133","Sunflower","MS",1.496,1.496]
["28135","Tallahatchie","MS",1.3489,1.3489]
["28137","Tate","MS",1.4599,1.4599]
["28139","Tippah","MS",1.2487,1.2487]
["28141","Tishomingo","MS",1.3209,1.3209]
["28143","Tunica","MS",1.0469,1.0469]
["28145","Union","MS",1.3434,1.3434]
["28147","Walthall","MS",1.2085,1.2085]
["28149","Warren","MS",1.2422,1.2422]
["28151","Washington","MS",1.1414,1.1414]
["28153","Wayne","MS",1.28,1.28]
["28155","Webster","MS",1.3919,1.3919]
["28157","Wilkinson","MS",1.2211,1.2211]
["28159","Winston","MS",1.3351,1.3351]
["28161","Yalobusha","MS",1.3532,1.3532]
["28163","Yazoo","MS",1.3177,1.3177]
["29001","Adair","MO",1.4382,1.4382]
["29003","Andrew","MO",1.2995,1.2995]
["29005","Atchison","MO",1.2796,1.2796]
["29007","Audrain","MO",1.3735,1.3735]
["29009","Barry","MO",1.4326,1.4326]
["29011","Barton","MO",1.3241,1.3241]
["29013","Bates","MO",1.3362,1.3362]
["29015","Benton","MO",1.4179,1.4179]
["29017","Bollinger","MO",1.4726,1.4726]
["29019","Boone","MO",1.3897,1.3897]
["29021","Buchanan","MO",1.2914,1.2914]
["29023","Butler","MO",1.3949,1.3949]
["29025","Caldwell","MO",1.2857,1.2857]
["29027","Callaway","MO",1.3904,1.3904]
["29029","Camden","MO",1.4431,1.4431]
["29031","Cape Girardeau","MO",1.4055,1.4055]
["29033","Carroll","MO",1.2215,1.2215]
["29035","Carter","MO",1.48,1.48]
["29037","Cass","MO",1.2345,1.2345]
["29039","Cedar","MO",1.4208,1.4208]
["29041","Chariton","MO",1.4191,1.4191]
["29043","Christian","MO",1.4195,1.4195]
["29045","Clark","MO",1.441,1.441]
["29047","Clay","MO",1.3291,1.3291]
["29049","Clinton","MO",1.3187,1.3187]
["29051","Cole","MO",1.4039,1.4039]
["29053","Cooper","MO",1.4419,1.4419]
["29055","Crawford","MO",1.4191,1.4191]
["29057","Dade","MO",1.4301,1.4301]
["29059","Dallas","MO",1.4337,1.4337]
["29061","Daviess","MO",1.3441,1.3441]
["29063","Dekalb","MO",1.3642,1.3642]
["29065","Dent","MO",1.4618,1.4618]
["29067","Douglas","MO",1.4535,1.4535]
["29069","Dunklin","MO",1.3006,1.3006]
["29071","Franklin","MO",1.404,1.404]
["29073","Gasconade","MO",1.4079,1.4079]
["29075","Gentry","MO",1.3365,1.3365]
["29077","Greene","MO",1.4142,1.4142]
["29079","Grundy","MO",1.4132,1.4132]
["29081","Harrison","MO",1.3794,1.3794]
["29083","Henry","MO",1.354,1.354]
["29085","Hickory","MO",1.4631,1.4631]
["29087","Holt","MO",1.036,1.036]
["29089","Howard","MO",1.4576,1.4576]
["29091","Howell","MO",1.4475,1.4475]
["29093","Iron","MO",1.3717,1.3717]
["29095","Jackson","MO",1.2725,1.2725]
["29097","Jasper","MO",1.3816,1.3816]
["29099","Jefferson","MO",1.4221,1.4221]
["29101","Johnson","MO",1.342,1.342]
["29103","Knox","MO",1.4311,1.4311]
["29105","Laclede","MO",1.4345,1.4345]
["29107","Lafayette","MO",1.2726,1.2726]
["29109","Lawrence","MO",1.3972,1.3972]
["29111","Lewis","MO",1.3972,1.3972]
["29113","Lincoln","MO",1.4084,1.4084]
["29115","Linn","MO",1.3737,1.3737]
["29117","Livingston","MO",1.3932,1.3932]
["29119","Mcdonald","MO",1.4465,1.4465]
["29121","Macon","MO",1.4205,1.4205]
["29123","Madison","MO",1.4762,1.4762]
["29125","Maries","MO",1.4246,1.4246]
["29127","Marion","MO",1.3797,1.3797]
["29129","Mercer","MO",1.2261,1.2261]
["29131","Miller","MO",1.4178,1.4178]
["29133","Mississippi","MO",1.4177,1.4177]
["29135","Moniteau","MO",1.3116,1.3116]
["29137","Monroe","MO",1.4536,1.4536]
["29139","Montgomery","MO",1.421,1.421]
["29141","Morgan","MO",1.4111,1.4111]
["29143","New Madrid","MO",1.3696,1.3696]
["29145","Newton","MO",1.4368,1.4368]
["29147","Nodaway","MO",1.3077,1.3077]
["29149","Oregon","MO",1.4841,1.4841]
["29151","Osage","MO",1.4237,1.4237]
["29153","Ozark","MO",1.4782,1.4782]
["29155","Pemiscot","MO",1.2035,1.2035]
["29157","Perry","MO",1.4271,1.4271]
["29159","Pettis","MO",1.3704,1.3704]
["29161","Phelps","MO",1.3918,1.3918]
["29163","Pike","MO",1.4499,1.4499]
["29165","Platte","MO",1.2614,1.2614]
["29167","Polk","MO",1.4306,1.4306]
["29169","Pulaski","MO",1.4438,1.4438]
["29171","Putnam","MO",1.5168,1.5168]
["29173","Ralls","MO",1.3366,1.3366]
["29175","Randolph","MO",1.3901,1.3901]
["29177","Ray","MO",1.2685,1.2685]
["29179","Reynolds","MO",1.4684,1.4684]
["29181","Ripley","MO",1.466,1.466]
["29183","St Charles","MO",1.4007,1.4007]
["29185","St Clair","MO",1.323,1.323]
["29186","Ste Genevieve","MO",1.4174,1.4174]
["29187","St Francois","MO",1.4427,1.4427]
["29189","St Louis","MO",1.3771,1.3771]
["29195","Saline","MO",1.3947,1.3947]
["29197","Schuyler","MO",1.3946,1.3946]
["29199","Scotland","MO",1.3846,1.3846]
["29201","Scott","MO",1.3586,1.3586]
["29203","Shannon","MO",1.4672,1.4672]
["29205","Shelby","MO",1.4415,1.4415]
["29207","Stoddard","MO",1.4339,1.4339]
["29209","Stone","MO",1.4575,1.4575]
["29211","Sullivan","MO",1.4487,1.4487]
["29213","Taney","MO",1.4172,1.4172]
["29215","Texas","MO",1.4746,1.4746]
["29217","Vernon","MO",1.407,1.407]
["29219","Warren","MO",1.4298,1.4298]
["29221","Washington","MO",1.4603,1.4603]
["29223","Wayne","MO",1.4535,1.4535]
["29225","Webster","MO",1.4667,1.4667]
["29227","Worth","MO",1.24,1.24]
["29229","Wright","MO",1.4499,1.4499]
["29510","St Louis City","MO",1.3006,1.3006]
["30001","Beaverhead","MT",1.017,1.017]
["30003","Big Horn","MT",1.0276,1.0276]
["30005","Blaine","MT",1.0276,1.0276]
["30007","Broadwater","MT",1.017,1.017]
["30009","Carbon","MT",1.017,1.017]
["30011","Carter","MT",1.017,1.017]
["30013","Cascade","MT",1.017,1.017]
["30015","Chouteau","MT",1.017,1.017]
["30017","Custer","MT",1.0276,1.0276]
["30019","Daniels","MT",1.0276,1.0276]
["30021","Dawson","MT",1.0276,1.0276]
["30023","Deer Lodge","MT",1.017,1.017]
["30025","Fallon","MT",1.0276,1.0276]
["30027","Fergus","MT",1.017,1.017]
["30029","Flathead","MT",1.0037,1.0037]
["30031","Gallatin","MT",1.017,1.017]
["30033","Garfield","MT",1.0276,1.0276]
["30035","Glacier","MT",1.017,1.017]
["30037","Golden Valley","MT",1.017,1.017]
["30039","Granite","MT",1.017,1.017]
["30041","Hill","MT",1.0276,1.0276]
["30043","Jefferson","MT",0.9926,0.9926]
["30045","Judith Basin","MT",1.017,1.017]
["30047","Lake","MT",1.0171,1.0171]
["30049","Lewis and Clark","MT",1.017,1.017]
["30051","Liberty","MT",1.0276,1.0276]
["30053","Lincoln","MT",1.0056,1.0056]
["30055","McCone","MT",1.0276,1.0276]
["30057","Madison","MT",1.017,1.017]
["30059","Meagher","MT",0.9942,0.9942]
["30061","Mineral","MT",1.017,1.017]
["30063","Missoula","MT",1.017,1.017]
["30065","Musselshell","MT",1.0276,1.0276]
["30067","Park","MT",1.017,1.017]
["30069","Petroleum","MT",1.0276,1.0276]
["30071","Phillips","MT",1.0276,1.0276]
["30073","Pondera","MT",1.017,1.017]
["30075","Powder River","MT",1.017,1.017]
["30077","Powell","MT",1.017,1.017]
["30079","Prairie","MT",1.0276,1.0276]
["30081","Ravalli","MT",1.017,1.017]
["30083","Richland","MT",1.0276,1.0276]
["30085","Roosevelt","MT",1.0276,1.0276]
["30087","Rosebud","MT",1.017,1.017]
["30089","Sanders","MT",1.017,1.017]
["30091","Sheridan","MT",1.0276,1.0276]
["30093","Silver Bow","MT",1.017,1.017]
["30095","Stillwater","MT",1.017,1.017]
["30097","Sweet Grass","MT",1.017,1.017]
["30099","Teton","MT",1.017,1.017]
["30101","Toole","MT",1.0276,1.0276]
["30103","Treasure","MT",1.0276,1.0276]
["30105","Valley","MT",1.0276,1.0276]
["30107","Wheatland","MT",1.017,1.017]
["30109","Wibaux","MT",1.0276,1.0276]
["30111","Yellowstone","MT",1.0276,1.0276]
["31001","Adams","NE",1.2145,1.2145]
["31003","Antelope","NE",1.1931,1.1931]
["31005","Arthur","NE",1.3006,1.3006]
["31007","Banner","NE",1.24,1.24]
["31009","Blaine","NE",1.3471,1.3471]
["31011","Boone","NE",1.2318,1.2318]
["31013","Box Butte","NE",1.094,1.094]
["31015","Boyd","NE",1.2768,1.2768]
["31017","Brown","NE",1.24,1.24]
["31019","Buffalo","NE",1.2768,1.2768]
["31021","Burt","NE",1.24,1.24]
["31023","Butler","NE",0.9492,0.9492]
["31025","Cass","NE",1.2426,1.2426]
["31027","Cedar","NE",1.2069,1.2069]
["31029","Chase","NE",1.24,1.24]
["31031","Cherry","NE",1.2252,1.2252]
["31033","Cheyenne","NE",1.24,1.24]
["31035","Clay","NE",1.1627,1.1627]
["31037","Colfax","NE",1.2062,1.2062]
["31039","Cuming","NE",1.3006,1.3006]
["31041","Custer","NE",1.3266,1.3266]
["31043","Dakota","NE",1.1978,1.1978]
["31045","Dawes","NE",1.2712,1.2712]
["31047","Dawson","NE",1.2489,1.2489]
["31049","Deuel","NE",1.3006,1.3006]
["31051","Dixon","NE",1.24,1.24]
["31053","Dodge","NE",1.1644,1.1644]
["31055","Douglas","NE",1.2158,1.2158]
["31057","Dundy","NE",1.3006,1.3006]
["31059","Fillmore","NE",1.3006,1.3006]
["31061","Franklin","NE",1.16,1.16]
["31063","Frontier","NE",1.234,1.234]
["31065","Furnas","NE",1.3006,1.3006]
["31067","Gage","NE",1.4015,1.4015]
["31069","Garden","NE",1.3006,1.3006]
["31071","Garfield","NE",1.2325,1.2325]
["31073","Gosper","NE",1.3006,1.3006]
["31075","Grant","NE",1.3006,1.3006]
["31077","Greeley","NE",1.3006,1.3006]
["31079","Hall","NE",1.193,1.193]
["31081","Hamilton","NE",1.0653,1.0653]
["31083","Harlan","NE",1.17,1.17]
["31085","Hayes","NE",1.3006,1.3006]
["31087","Hitchcock","NE",1.3006,1.3006]
["31089","Holt","NE",1.1148,1.1148]
["31091","Hooker","NE",1.1292,1.1292]
["31093","Howard","NE",1.1046,1.1046]
["31095","Jefferson","NE",1.3006,1.3006]
["31097","Johnson","NE",1.3006,1.3006]
["31099","Kearney","NE",1.3006,1.3006]
["31101","Keith","NE",1.3006,1.3006]
["31103","Keya Paha","NE",0.924,0.924]
["31105","Kimball","NE",1.24,1.24]
["31107","Knox","NE",1.2325,1.2325]
["31109","Lancaster","NE",1.2504,1.2504]
["31111","Lincoln","NE",1.2012,1.2012]
["31113","Logan","NE",1.3006,1.3006]
["31115","Loup","NE",1.3006,1.3006]
["31117","McPherson","NE",1.3006,1.3006]
["31119","Madison","NE",1.2131,1.2131]
["31121","Merrick","NE",1.3006,1.3006]
["31123","Morrill","NE",0.9483,0.9483]
["31125","Nance","NE",1.3006,1.3006]
["31127","Nemaha","NE",1.1356,1.1356]
["31129","Nuckolls","NE",1.3006,1.3006]
["31131","Otoe","NE",1.2492,1.2492]
["31133","Pawnee","NE",1.2022,1.2022]
["31135","Perkins","NE",1.3006,1.3006]
["31137","Phelps","NE",1.0042,1.0042]
["31139","Pierce","NE",1.3006,1.3006]
["31141","Platte","NE",1.2479,1.2479]
["31143","Polk","NE",1.2125,1.2125]
["31145","Red Willow","NE",1.2239,1.2239]
["31147","Richardson","NE",1.3128,1.3128]
["31149","Rock","NE",1.3006,1.3006]
["31151","Saline","NE",1.2023,1.2023]
["31153","Sarpy","NE",1.2081,1.2081]
["31155","Saunders","NE",1.3192,1.3192]
["31157","Scotts Bluff","NE",1.2321,1.2321]
["31159","Seward","NE",1.2175,1.2175]
["31161","Sheridan","NE",1.3006,1.3006]
["31163","Sherman","NE",1.3006,1.3006]
["31165","Sioux","NE",1.3006,1.3006]
["31167","Stanton","NE",1.1136,1.1136]
["31169","Thayer","NE",1.24,1.24]
["31171","Thomas","NE",1.3006,1.3006]
["31173","Thurston","NE",1.2858,1.2858]
["31175","Valley","NE",1.3006,1.3006]
["31177","Washington","NE",1.1333,1.1333]
["31179","Wayne","NE",1.2858,1.2858]
["31181","Webster","NE",1.0512,1.0512]
["31183","Wheeler","NE",1.3006,1.3006]
["31185","York","NE",1.2926,1.2926]
["32001","Churchill","NV",1.0276,1.0276]
["32003","Clark","NV",1.0276,1.0276]
["32005","Douglas","NV",1.0276,1.0276]
["32007","Elko","NV",1.0276,1.0276]
["32009","Esmeralda","NV",1.0276,1.0276]
["32011","Eureka","NV",1.0276,1.0276]
["32013","Humboldt","NV",1.0276,1.0276]
["32015","Lander","NV",1.0276,1.0276]
["32017","Lincoln","NV",1.0276,1.0276]
["32019","Lyon","NV",1.0276,1.0276]
["32021","Mineral","NV",1.0276,1.0276]
["32023","Nye","NV",1.0276,1.0276]
["32027","Pershing","NV",1.0276,1.0276]
["32029","Storey","NV",1.0276,1.0276]
["32031","Washoe","NV",1.0276,1.0276]
["32033","White Pine","NV",1.0276,1.0276]
["32510","Carson City","NV",1.0154,1.0154]
["33001","Belknap","NH",1.2206,1.2206]
["33003","Carroll","NH",1.3142,1.3142]
["33005","Cheshire","NH",1.2371,1.2371]
["33007","Coos","NH",1.2233,1.2233]
["33009","Grafton","NH",1.2363,1.2363]
["33011","Hillsborough","NH",1.2197,1.2197]
["33013","Merrimack","NH",1.2001,1.2001]
["33015","Rockingham","NH",1.2164,1.2164]
["33017","Strafford","NH",1.1751,1.1751]
["33019","Sullivan","NH",1.2215,1.2215]
["34001","Atlantic","NJ",1.2837,1.2837]
["34003","Bergen","NJ",1.1964,1.1964]
["34005","Burlington","NJ",1.366,1.366]
["34007","Camden","NJ",1.448,1.448]
["34009","Cape May","NJ",1.2832,1.2832]
["34011","Cumberland","NJ",1.2976,1.2976]
["34013","Essex","NJ",1.2934,1.2934]
["34015","Gloucester","NJ",1.2739,1.2739]
["34017","Hudson","NJ",1.2934,1.2934]
["34019","Hunterdon","NJ",1.313,1.313]
["34021","Mercer","NJ",1.3445,1.3445]
["34023","Middlesex","NJ",1.3559,1.3559]
["34025","Monmouth","NJ",1.3465,1.3465]
["34027","Morris","NJ",1.2817,1.2817]
["34029","Ocean","NJ",1.3534,1.3534]
["34031","Passaic","NJ",1.0005,1.0005]
["34033","Salem","NJ",1.3075,1.3075]
["34035","Somerset","NJ",1.2066,1.2066]
["34037","Sussex","NJ",1.3751,1.3751]
["34039","Union","NJ",1.2934,1.2934]
["34041","Warren","NJ",1.3707,1.3707]
["35001","Bernalillo","NM",1.017,1.017]
["35003","Catron","NM",1.0383,1.0383]
["35005","Chaves","NM",1.017,1.017]
["35006","Cibola","NM",1.017,1.017]
["35007","Colfax","NM",1.0199,1.0199]
["35009","Curry","NM",1.0276,1.0276]
["35011","De Baca","NM",1.0276,1.0276]
["35013","Dona Ana","NM",1.0276,1.0276]
["35015","Eddy","NM",1.017,1.017]
["35017","Grant","NM",1.0557,1.0557]
["35019","Guadalupe","NM",1.0276,1.0276]
["35021","Harding","NM",1.0276,1.0276]
["35023","Hidalgo","NM",1.0557,1.0557]
["35025","Lea","NM",1.0276,1.0276]
["35027","Lincoln","NM",1.017,1.017]
["35028","Los Alamos","NM",1.0187,1.0187]
["35029","Luna","NM",1.0276,1.0276]
["35031","Mckinley","NM",1.017,1.017]
["35033","Mora","NM",1.0173,1.0173]
["35035","Otero","NM",1.02,1.02]
["35037","Quay","NM",1.0276,1.0276]
["35039","Rio Arriba","NM",1.0179,1.0179]
["35041","Roosevelt","NM",1.0276,1.0276]
["35043","Sandoval","NM",1.0186,1.0186]
["35045","San Juan","NM",1.0276,1.0276]
["35047","San Miguel","NM",1.0198,1.0198]
["35049","Santa Fe","NM",1.0091,1.0091]
["35051","Sierra","NM",1.0357,1.0357]
["35053","Socorro","NM",1.0175,1.0175]
["35055","Taos","NM",1.0198,1.0198]
["35057","Torrance","NM",1.0174,1.0174]
["35059","Union","NM",1.0276,1.0276]
["35061","Valencia","NM",1.017,1.017]
["36001","Albany","NY",1.3659,1.3659]
["36003","Allegany","NY",1.3822,1.3822]
["36005","Bronx","NY",1.2934,1.2934]
["36007","Broome","NY",1.3164,1.3164]
["36009","Cattaraugus","NY",1.3823,1.3823]
["36011","Cayuga","NY",1.2821,1.2821]
["36013","Chautauqua","NY",1.3823,1.3823]
["36015","Chemung","NY",1.3165,1.3165]
["36017","Chenango","NY",1.3163,1.3163]
["36019","Clinton","NY",1.3004,1.3004]
["36021","Columbia","NY",1.3646,1.3646]
["36023","Cortland","NY",1.3163,1.3163]
["36025","Delaware","NY",1.3164,1.3164]
["36027","Dutchess","NY",1.3582,1.3582]
["36029","Erie","NY",1.2823,1.2823]
["36031","Essex","NY",1.3456,1.3456]
["36033","Franklin","NY",1.3005,1.3005]
["36035","Fulton","NY",1.3054,1.3054]
["36037","Genesee","NY",1.2825,1.2825]
["36039","Greene","NY",1.3585,1.3585]
["36041","Hamilton","NY",1.3457,1.3457]
["36043","Herkimer","NY",1.3054,1.3054]
["36045","Jefferson","NY",1.3004,1.3004]
["36047","Kings","NY",1.2934,1.2934]
["36049","Lewis","NY",1.3054,1.3054]
["36051","Livingston","NY",1.2822,1.2822]
["36053","Madison","NY",1.282,1.282]
["36055","Monroe","NY",1.2825,1.2825]
["36057","Montgomery","NY",1.3655,1.3655]
["36059","Nassau","NY",1.3719,1.3719]
["36061","New York","NY",1.2934,1.2934]
["36063","Niagara","NY",1.2773,1.2773]
["36065","Oneida","NY",1.3054,1.3054]
["36067","Onondaga","NY",1.2823,1.2823]
["36069","Ontario","NY",1.2821,1.2821]
["36071","Orange","NY",1.3589,1.3589]
["36073","Orleans","NY",1.2823,1.2823]
["36075","Oswego","NY",1.2821,1.2821]
["36077","Otsego","NY",1.3162,1.3162]
["36079","Putnam","NY",1.359,1.359]
["36081","Queens","NY",1.2934,1.2934]
["36083","Rensselaer","NY",1.3646,1.3646]
["36085","Richmond","NY",1.3584,1.3584]
["36087","Rockland","NY",1.2934,1.2934]
["36089","St Lawrence","NY",1.3004,1.3004]
["36091","Saratoga","NY",1.3648,1.3648]
["36093","Schenectady","NY",1.3679,1.3679]
["36095","Schoharie","NY",1.3583,1.3583]
["36097","Schuyler","NY",1.3156,1.3156]
["36099","Seneca","NY",1.2823,1.2823]
["36101","Steuben","NY",1.3823,1.3823]
["36103","Suffolk","NY",1.2934,1.2934]
["36105","Sullivan","NY",1.3585,1.3585]
["36107","Tioga","NY",1.3164,1.3164]
["36109","Tompkins","NY",1.3164,1.3164]
["36111","Ulster","NY",1.3583,1.3583]
["36113","Warren","NY",1.3456,1.3456]
["36115","Washington","NY",1.3649,1.3649]
["36117","Wayne","NY",1.2817,1.2817]
["36119","Westchester","NY",1.359,1.359]
["36121","Wyoming","NY",1.2821,1.2821]
["36123","Yates","NY",1.282,1.282]
["37001","Alamance","NC",1.2195,1.2195]
["37003","Alexander","NC",1.2559,1.2559]
["37005","Alleghany","NC",1.1703,1.1703]
["37007","Anson","NC",1.2996,1.2996]
["37009","Ashe","NC",1.2649,1.2649]
["37011","Avery","NC",1.1996,1.1996]
["37013","Beaufort","NC",1.2008,1.2008]
["37015","Bertie","NC",1.1973,1.1973]
["37017","Bladen","NC",1.2052,1.2052]
["37019","Brunswick","NC",1.2427,1.2427]
["37021","Buncombe","NC",1.2342,1.2342]
["37023","Burke","NC",1.2569,1.2569]
["37025","Cabarrus","NC",1.289,1.289]
["37027","Caldwell","NC",1.2951,1.2951]
["37029","Camden","NC",1.1375,1.1375]
["37031","Carteret","NC",1.1046,1.1046]
["37033","Caswell","NC",1.1775,1.1775]
["37035","Catawba","NC",1.3113,1.3113]
["37037","Chatham","NC",1.2312,1.2312]
["37039","Cherokee","NC",1.4025,1.4025]
["37041","Chowan","NC",1.1858,1.1858]
["37043","Clay","NC",1.1702,1.1702]
["37045","Cleveland","NC",1.339,1.339]
["37047","Columbus","NC",1.2595,1.2595]
["37049","Craven","NC",1.1899,1.1899]
["37051","Cumberland","NC",1.1003,1.1003]
["37053","Currituck","NC",1.191,1.191]
["37055","Dare","NC",1.546,1.546]
["37057","Davidson","NC",1.1825,1.1825]
["37059","Davie","NC",1.3412,1.3412]
["37061","Duplin","NC",1.2238,1.2238]
["37063","Durham","NC",1.2935,1.2935]
["37065","Edgecombe","NC",1.229,1.229]
["37067","Forsyth","NC",1.0425,1.0425]
["37069","Franklin","NC",1.3079,1.3079]
["37071","Gaston","NC",1.2001,1.2001]
["37073","Gates","NC",1.164,1.164]
["37075","Graham","NC",1.3533,1.3533]
["37077","Granville","NC",1.2137,1.2137]
["37079","Greene","NC",1.2602,1.2602]
["37081","Guilford","NC",1.0669,1.0669]
["37083","Halifax","NC",1.239,1.239]
["37085","Harnett","NC",1.2304,1.2304]
["37087","Haywood","NC",1.1591,1.1591]
["37089","Henderson","NC",1.3164,1.3164]
["37091","Hertford","NC",1.331,1.331]
["37093","Hoke","NC",1.2505,1.2505]
["37095","Hyde","NC",1.0997,1.0997]
["37097","Iredell","NC",1.2521,1.2521]
["37099","Jackson","NC",1.258,1.258]
["37101","Johnston","NC",1.2424,1.2424]
["37103","Jones","NC",1.2226,1.2226]
["37105","Lee","NC",1.2815,1.2815]
["37107","Lenoir","NC",1.2072,1.2072]
["37109","Lincoln","NC",1.2899,1.2899]
["37111","McDowell","NC",1.3312,1.3312]
["37113","Macon","NC",1.3778,1.3778]
["37115","Madison","NC",0.9989,0.9989]
["37117","Martin","NC",1.1908,1.1908]
["37119","Mecklenburg","NC",1.1763,1.1763]
["37121","Mitchell","NC",1.1373,1.1373]
["37123","Montgomery","NC",1.2571,1.2571]
["37125","Moore","NC",1.2272,1.2272]
["37127","Nash","NC",1.1703,1.1703]
["37129","New Hanover","NC",1.346,1.346]
["37131","Northampton","NC",1.3173,1.3173]
["37133","Onslow","NC",1.258,1.258]
["37135","Orange","NC",1.1537,1.1537]
["37137","Pamlico","NC",1.1334,1.1334]
["37139","Pasquotank","NC",1.2471,1.2471]
["37141","Pender","NC",1.2462,1.2462]
["37143","Perquimans","NC",1.3445,1.3445]
["37145","Person","NC",1.2281,1.2281]
["37147","Pitt","NC",1.1857,1.1857]
["37149","Polk","NC",1.4577,1.4577]
["37151","Randolph","NC",1.388,1.388]
["37153","Richmond","NC",1.2571,1.2571]
["37155","Robeson","NC",1.2391,1.2391]
["37157","Rockingham","NC",1.3171,1.3171]
["37159","Rowan","NC",1.1938,1.1938]
["37161","Rutherford","NC",1.1908,1.1908]
["37163","Sampson","NC",1.2619,1.2619]
["37165","Scotland","NC",1.1432,1.1432]
["37167","Stanly","NC",1.3324,1.3324]
["37169","Stokes","NC",1.2339,1.2339]
["37171","Surry","NC",1.2597,1.2597]
["37173","Swain","NC",1.4391,1.4391]
["37175","Transylvania","NC",1.1868,1.1868]
["37177","Tyrrell","NC",1.086,1.086]
["37179","Union","NC",1.362,1.362]
["37181","Vance","NC",1.2081,1.2081]
["37183","Wake","NC",1.1694,1.1694]
["37185","Warren","NC",1.2178,1.2178]
["37187","Washington","NC",1.0723,1.0723]
["37189","Watauga","NC",1.243,1.243]
["37191","Wayne","NC",1.3201,1.3201]
["37193","Wilkes","NC",1.1995,1.1995]
["37195","Wilson","NC",1.3036,1.3036]
["37197","Yadkin","NC",1.3609,1.3609]
["37199","Yancey","NC",1.2904,1.2904]
["38001","Adams","ND",1.3006,1.3006]
["38003","Barnes","ND",1.3006,1.3006]
["38005","Benson","ND",1.2036,1.2036]
["38007","Billings","ND",1.3006,1.3006]
["38009","Bottineau","ND",1.19,1.19]
["38011","Bowman","ND",1.3006,1.3006]
["38013","Burke","ND",1.1946,1.1946]
["38015","Burleigh","ND",1.2877,1.2877]
["38017","Cass","ND",1.2052,1.2052]
["38019","Cavalier","ND",1.2888,1.2888]
["38021","Dickey","ND",1.1742,1.1742]
["38023","Divide","ND",1.24,1.24]
["38025","Dunn","ND",1.3006,1.3006]
["38027","Eddy","ND",1.3006,1.3006]
["38029","Emmons","ND",1.3006,1.3006]
["38031","Foster","ND",1.1746,1.1746]
["38033","Golden Valley","ND",1.3006,1.3006]
["38035","Grand Forks","ND",1.1514,1.1514]
["38037","Grant","ND",1.3006,1.3006]
["38039","Griggs","ND",1.3006,1.3006]
["38041","Hettinger","ND",1.24,1.24]
["38043","Kidder","ND",0.924,0.924]
["38045","Lamoure","ND",1.1209,1.1209]
["38047","Logan","ND",1.3006,1.3006]
["38049","McHenry","ND",1.017,1.017]
["38051","McIntosh","ND",1.1742,1.1742]
["38053","Mckenzie","ND",1.2369,1.2369]
["38055","Mclean","ND",1.2126,1.2126]
["38057","Mercer","ND",1.24,1.24]
["38059","Morton","ND",0.924,0.924]
["38061","Mountrail","ND",1.1913,1.1913]
["38063","Nelson","ND",1.0956,1.0956]
["38065","Oliver","ND",1.3006,1.3006]
["38067","Pembina","ND",1.1743,1.1743]
["38069","Pierce","ND",1.3006,1.3006]
["38071","Ramsey","ND",1.2214,1.2214]
["38073","Ransom","ND",1.2582,1.2582]
["38075","Renville","ND",1.3006,1.3006]
["38077","Richland","ND",1.2039,1.2039]
["38079","Rolette","ND",1.3006,1.3006]
["38081","Sargent","ND",1.3006,1.3006]
["38083","Sheridan","ND",1.1156,1.1156]
["38085","Sioux","ND",0.924,0.924]
["38087","Slope","ND",1.3006,1.3006]
["38089","Stark","ND",1.1208,1.1208]
["38091","Steele","ND",1.24,1.24]
["38093","Stutsman","ND",1.2076,1.2076]
["38095","Towner","ND",1.3006,1.3006]
["38097","Traill","ND",1.1259,1.1259]
["38099","Walsh","ND",1.2159,1.2159]
["38101","Ward","ND",1.1844,1.1844]
["38103","Wells","ND",1.3006,1.3006]
["38105","Williams","ND",1.2731,1.2731]
["39001","Adams","OH",1.3681,1.3681]
["39003","Allen","OH",1.3334,1.3334]
["39005","Ashland","OH",1.3222,1.3222]
["39007","Ashtabula","OH",1.3224,1.3224]
["39009","Athens","OH",1.3229,1.3229]
["39011","Auglaize","OH",1.3333,1.3333]
["39013","Belmont","OH",1.2917,1.2917]
["39015","Brown","OH",1.3688,1.3688]
["39017","Butler","OH",1.3692,1.3692]
["39019","Carroll","OH",1.2878,1.2878]
["39021","Champaign","OH",1.3688,1.3688]
["39023","Clark","OH",1.3698,1.3698]
["39025","Clermont","OH",1.3765,1.3765]
["39027","Clinton","OH",1.3699,1.3699]
["39029","Columbiana","OH",1.3223,1.3223]
["39031","Coshocton","OH",1.2879,1.2879]
["39033","Crawford","OH",1.333,1.333]
["39035","Cuyahoga","OH",1.3216,1.3216]
["39037","Darke","OH",1.3687,1.3687]
["39039","Defiance","OH",1.3336,1.3336]
["39041","Delaware","OH",1.3341,1.3341]
["39043","Erie","OH",1.3246,1.3246]
["39045","Fairfield","OH",1.3697,1.3697]
["39047","Fayette","OH",1.3006,1.3006]
["39049","Franklin","OH",1.383,1.383]
["39051","Fulton","OH",1.3006,1.3006]
["39053","Gallia","OH",1.368,1.368]
["39055","Geauga","OH",1.3226,1.3226]
["39057","Greene","OH",1.3693,1.3693]
["39059","Guernsey","OH",1.2879,1.2879]
["39061","Hamilton","OH",1.3715,1.3715]
["39063","Hancock","OH",1.3324,1.3324]
["39065","Hardin","OH",1.3326,1.3326]
["39067","Harrison","OH",1.3124,1.3124]
["39069","Henry","OH",1.392,1.392]
["39071","Highland","OH",1.3684,1.3684]
["39073","Hocking","OH",1.3229,1.3229]
["39075","Holmes","OH",1.288,1.288]
["39077","Huron","OH",1.3223,1.3223]
["39079","Jackson","OH",1.3681,1.3681]
["39081","Jefferson","OH",1.2881,1.2881]
["39083","Knox","OH",1.3343,1.3343]
["39085","Lake","OH",1.3221,1.3221]
["39087","Lawrence","OH",1.3672,1.3672]
["39089","Licking","OH",1.3695,1.3695]
["39091","Logan","OH",1.3334,1.3334]
["39093","Lorain","OH",1.3216,1.3216]
["39095","Lucas","OH",1.3322,1.3322]
["39097","Madison","OH",1.3754,1.3754]
["39099","Mahoning","OH",1.3223,1.3223]
["39101","Marion","OH",1.334,1.334]
["39103","Medina","OH",1.322,1.322]
["39105","Meigs","OH",1.3228,1.3228]
["39107","Mercer","OH",1.3332,1.3332]
["39109","Miami","OH",1.3718,1.3718]
["39111","Monroe","OH",1.2875,1.2875]
["39113","Montgomery","OH",1.3006,1.3006]
["39115","Morgan","OH",1.3221,1.3221]
["39117","Morrow","OH",1.3315,1.3315]
["39119","Muskingum","OH",1.288,1.288]
["39121","Noble","OH",1.2884,1.2884]
["39123","Ottawa","OH",1.3321,1.3321]
["39125","Paulding","OH",1.3488,1.3488]
["39127","Perry","OH",1.3229,1.3229]
["39129","Pickaway","OH",1.3693,1.3693]
["39131","Pike","OH",1.3551,1.3551]
["39133","Portage","OH",1.3223,1.3223]
["39135","Preble","OH",1.3698,1.3698]
["39137","Putnam","OH",1.3006,1.3006]
["39139","Richland","OH",1.3223,1.3223]
["39141","Ross","OH",1.368,1.368]
["39143","Sandusky","OH",1.3331,1.3331]
["39145","Scioto","OH",1.368,1.368]
["39147","Seneca","OH",1.3322,1.3322]
["39149","Shelby","OH",1.3006,1.3006]
["39151","Stark","OH",1.3221,1.3221]
["39153","Summit","OH",1.3221,1.3221]
["39155","Trumbull","OH",1.3221,1.3221]
["39157","Tuscarawas","OH",1.2879,1.2879]
["39159","Union","OH",1.3332,1.3332]
["39161","Van Wert","OH",1.3006,1.3006]
["39163","Vinton","OH",1.3229,1.3229]
["39165","Warren","OH",1.3706,1.3706]
["39167","Washington","OH",1.3227,1.3227]
["39169","Wayne","OH",1.3227,1.3227]
["39171","Williams","OH",1.3348,1.3348]
["39173","Wood","OH",1.3343,1.3343]
["39175","Wyandot","OH",1.3321,1.3321]
["40001","Adair","OK",1.4572,1.4572]
["40003","Alfalfa","OK",1.2906,1.2906]
["40005","Atoka","OK",1.3691,1.3691]
["40007","Beaver","OK",1.2906,1.2906]
["40009","Beckham","OK",1.2906,1.2906]
["40011","Blaine","OK",1.2906,1.2906]
["40013","Bryan","OK",1.3828,1.3828]
["40015","Caddo","OK",1.2906,1.2906]
["40017","Canadian","OK",1.2906,1.2906]
["40019","Carter","OK",1.2906,1.2906]
["40021","Cherokee","OK",1.4203,1.4203]
["40023","Choctaw","OK",1.4091,1.4091]
["40025","Cimarron","OK",1.2906,1.2906]
["40027","Cleveland","OK",1.2906,1.2906]
["40029","Coal","OK",1.2906,1.2906]
["40031","Comanche","OK",1.2906,1.2906]
["40033","Cotton","OK",1.2906,1.2906]
["40035","Craig","OK",1.2906,1.2906]
["40037","Creek","OK",1.2906,1.2906]
["40039","Custer","OK",1.2906,1.2906]
["40041","Delaware","OK",1.4291,1.4291]
["40043","Dewey","OK",1.2906,1.2906]
["40045","Ellis","OK",1.2906,1.2906]
["40047","Garfield","OK",1.2906,1.2906]
["40049","Garvin","OK",1.2906,1.2906]
["40051","Grady","OK",1.2906,1.2906]
["40053","Grant","OK",1.2906,1.2906]
["40055","Greer","OK",1.2906,1.2906]
["40057","Harmon","OK",1.2906,1.2906]
["40059","Harper","OK",1.2906,1.2906]
["40061","Haskell","OK",1.4109,1.4109]
["40063","Hughes","OK",1.2906,1.2906]
["40065","Jackson","OK",1.2906,1.2906]
["40067","Jefferson","OK",1.2906,1.2906]
["40069","Johnston","OK",1.2906,1.2906]
["40071","Kay","OK",1.2906,1.2906]
["40073","Kingfisher","OK",1.2906,1.2906]
["40075","Kiowa","OK",1.2906,1.2906]
["40077","Latimer","OK",1.4214,1.4214]
["40079","Le Flore","OK",1.3991,1.3991]
["40081","Lincoln","OK",1.2906,1.2906]
["40083","Logan","OK",1.2906,1.2906]
["40085","Love","OK",1.2906,1.2906]
["40087","Mcclain","OK",1.2906,1.2906]
["40089","McCurtain","OK",1.4091,1.4091]
["40091","McIntosh","OK",1.2906,1.2906]
["40093","Major","OK",1.2906,1.2906]
["40095","Marshall","OK",1.2906,1.2906]
["40097","Mayes","OK",1.4581,1.4581]
["40099","Murray","OK",1.2906,1.2906]
["40101","Muskogee","OK",1.2906,1.2906]
["40103","Noble","OK",1.2906,1.2906]
["40105","Nowata","OK",1.2906,1.2906]
["40107","Okfuskee","OK",1.2906,1.2906]
["40109","Oklahoma","OK",1.2906,1.2906]
["40111","Okmulgee","OK",1.2906,1.2906]
["40113","Osage","OK",1.2906,1.2906]
["40115","Ottawa","OK",1.4903,1.4903]
["40117","Pawnee","OK",1.2906,1.2906]
["40119","Payne","OK",1.2906,1.2906]
["40121","Pittsburg","OK",1.4558,1.4558]
["40123","Pontotoc","OK",1.2906,1.2906]
["40125","Pottawatomie","OK",1.2906,1.2906]
["40127","Pushmataha","OK",1.4104,1.4104]
["40129","Roger Mills","OK",1.2906,1.2906]
["40131","Rogers","OK",1.2906,1.2906]
["40133","Seminole","OK",1.2906,1.2906]
["40135","Sequoyah","OK",1.4791,1.4791]
["40137","Stephens","OK",1.2906,1.2906]
["40139","Texas","OK",1.2906,1.2906]
["40141","Tillman","OK",1.2906,1.2906]
["40143","Tulsa","OK",1.2906,1.2906]
["40145","Wagoner","OK",1.2906,1.2906]
["40147","Washington","OK",1.2906,1.2906]
["40149","Washita","OK",1.2906,1.2906]
["40151","Woods","OK",1.2906,1.2906]
["40153","Woodward","OK",1.2906,1.2906]
["41001","Baker","OR",1.017,1.017]
["41003","Benton","OR",1.0271,1.0271]
["41005","Clackamas","OR",1.0265,1.0265]
["41007","Clatsop","OR",1.1548,1.1548]
["41009","Columbia","OR",1.0346,1.0346]
["41011","Coos","OR",1.0305,1.0305]
["41013","Crook","OR",1.017,1.017]
["41015","Curry","OR",1.0562,1.0562]
["41017","Deschutes","OR",1.017,1.017]
["41019","Douglas","OR",1.0267,1.0267]
["41021","Gilliam","OR",1.0276,1.0276]
["41023","Grant","OR",1.017,1.017]
["41025","Harney","OR",1.017,1.017]
["41027","Hood River","OR",1.017,1.017]
["41029","Jackson","OR",1.0197,1.0197]
["41031","Jefferson","OR",1.017,1.017]
["41033","Josephine","OR",1.0444,1.0444]
["41035","Klamath","OR",1.0227,1.0227]
["41037","Lake","OR",1.017,1.017]
["41039","Lane","OR",1.0268,1.0268]
["41041","Lincoln","OR",1.0424,1.0424]
["41043","Linn","OR",1.0266,1.0266]
["41045","Malheur","OR",1.0276,1.0276]
["41047","Marion","OR",1.017,1.017]
["41049","Morrow","OR",1.017,1.017]
["41051","Multnomah","OR",1.017,1.017]
["41053","Polk","OR",1.0424,1.0424]
["41055","Sherman","OR",1.0276,1.0276]
["41057","Tillamook","OR",1.027,1.027]
["41059","Umatilla","OR",1.017,1.017]
["41061","Union","OR",1.017,1.017]
["41063","Wallowa","OR",1.017,1.017]
["41065","Wasco","OR",1.017,1.017]
["41067","Washington","OR",1.0276,1.0276]
["41069","Wheeler","OR",1.0262,1.0262]
["41071","Yamhill","OR",1.0269,1.0269]
["42001","Adams","PA",1.3904,1.3904]
["42003","Allegheny","PA",1.2644,1.2644]
["42005","Armstrong","PA",1.2539,1.2539]
["42007","Beaver","PA",1.2644,1.2644]
["42009","Bedford","PA",1.3316,1.3316]
["42011","Berks","PA",1.3891,1.3891]
["42013","Blair","PA",1.344,1.344]
["42015","Bradford","PA",1.2691,1.2691]
["42017","Bucks","PA",1.3885,1.3885]
["42019","Butler","PA",1.2584,1.2584]
["42021","Cambria","PA",1.3396,1.3396]
["42023","Cameron","PA",1.2699,1.2699]
["42025","Carbon","PA",1.2264,1.2264]
["42027","Centre","PA",1.3259,1.3259]
["42029","Chester","PA",1.389,1.389]
["42031","Clarion","PA",1.3403,1.3403]
["42033","Clearfield","PA",1.2996,1.2996]
["42035","Clinton","PA",1.2681,1.2681]
["42037","Columbia","PA",1.2795,1.2795]
["42039","Crawford","PA",1.2603,1.2603]
["42041","Cumberland","PA",1.3945,1.3945]
["42043","Dauphin","PA",1.3796,1.3796]
["42045","Delaware","PA",1.3788,1.3788]
["42047","Elk","PA",1.2479,1.2479]
["42049","Erie","PA",1.2532,1.2532]
["42051","Fayette","PA",1.3531,1.3531]
["42053","Forest","PA",1.2399,1.2399]
["42055","Franklin","PA",1.3797,1.3797]
["42057","Fulton","PA",1.3405,1.3405]
["42059","Greene","PA",1.2639,1.2639]
["42061","Huntingdon","PA",1.3654,1.3654]
["42063","Indiana","PA",1.2634,1.2634]
["42065","Jefferson","PA",1.3186,1.3186]
["42067","Juniata","PA",1.371,1.371]
["42069","Lackawanna","PA",1.2781,1.2781]
["42071","Lancaster","PA",1.3909,1.3909]
["42073","Lawrence","PA",1.2598,1.2598]
["42075","Lebanon","PA",1.3992,1.3992]
["42077","Lehigh","PA",1.389,1.389]
["42079","Luzerne","PA",1.2798,1.2798]
["42081","Lycoming","PA",1.3247,1.3247]
["42083","McKean","PA",1.2291,1.2291]
["42085","Mercer","PA",1.2577,1.2577]
["42087","Mifflin","PA",1.3568,1.3568]
["42089","Monroe","PA",1.257,1.257]
["42091","Montgomery","PA",1.3886,1.3886]
["42093","Montour","PA",1.3272,1.3272]
["42095","Northampton","PA",1.3883,1.3883]
["42097","Northumberland","PA",1.3247,1.3247]
["42099","Perry","PA",1.3697,1.3697]
["42101","Philadelphia","PA",1.3904,1.3904]
["42103","Pike","PA",1.2645,1.2645]
["42105","Potter","PA",1.2061,1.2061]
["42107","Schuylkill","PA",1.2835,1.2835]
["42109","Snyder","PA",1.3679,1.3679]
["42111","Somerset","PA",1.334,1.334]
["42113","Sullivan","PA",1.2403,1.2403]
["42115","Susquehanna","PA",1.2408,1.2408]
["42117","Tioga","PA",1.2622,1.2622]
["42119","Union","PA",1.3661,1.3661]
["42121","Venango","PA",1.3265,1.3265]
["42123","Warren","PA",1.2429,1.2429]
["42125","Washington","PA",1.2639,1.2639]
["42127","Wayne","PA",1.2539,1.2539]
["42129","Westmoreland","PA",1.2641,1.2641]
["42131","Wyoming","PA",1.2659,1.2659]
["42133","York","PA",1.4009,1.4009]
["44001","Bristol","RI",1.2934,1.2934]
["44003","Kent","RI",1.4877,1.4877]
["44005","Newport","RI",0.9471,0.9471]
["44007","Providence","RI",1.4811,1.4811]
["44009","Washington","RI",1.4848,1.4848]
["45001","Abbeville","SC",1.2454,1.2454]
["45003","Aiken","SC",1.2751,1.2751]
["45005","Allendale","SC",1.3416,1.3416]
["45007","Anderson","SC",1.3765,1.3765]
["45009","Bamberg","SC",1.2686,1.2686]
["45011","Barnwell","SC",1.3746,1.3746]
["45013","Beaufort","SC",1.283,1.283]
["45015","Berkeley","SC",1.3015,1.3015]
["45017","Calhoun","SC",1.1945,1.1945]
["45019","Charleston","SC",1.3289,1.3289]
["45021","Cherokee","SC",1.3374,1.3374]
["45023","Chester","SC",1.27,1.27]
["45025","Chesterfield","SC",1.1987,1.1987]
["45027","Clarendon","SC",1.2549,1.2549]
["45029","Colleton","SC",1.2745,1.2745]
["45031","Darlington","SC",1.3313,1.3313]
["45033","Dillon","SC",1.2929,1.2929]
["45035","Dorchester","SC",1.2891,1.2891]
["45037","Edgefield","SC",1.2761,1.2761]
["45039","Fairfield","SC",1.1988,1.1988]
["45041","Florence","SC",1.291,1.291]
["45043","Georgetown","SC",1.3384,1.3384]
["45045","Greenville","SC",1.3496,1.3496]
["45047","Greenwood","SC",1.2855,1.2855]
["45049","Hampton","SC",1.2801,1.2801]
["45051","Horry","SC",1.2402,1.2402]
["45053","Jasper","SC",1.2832,1.2832]
["45055","Kershaw","SC",1.2726,1.2726]
["45057","Lancaster","SC",1.2187,1.2187]
["45059","Laurens","SC",1.2983,1.2983]
["45061","Lee","SC",1.3443,1.3443]
["45063","Lexington","SC",1.2751,1.2751]
["45065","McCormick","SC",1.3107,1.3107]
["45067","Marion","SC",1.2448,1.2448]
["45069","Marlboro","SC",1.2565,1.2565]
["45071","Newberry","SC",1.2567,1.2567]
["45073","Oconee","SC",1.3704,1.3704]
["45075","Orangeburg","SC",1.2362,1.2362]
["45077","Pickens","SC",1.2075,1.2075]
["45079","Richland","SC",1.2723,1.2723]
["45081","Saluda","SC",1.2477,1.2477]
["45083","Spartanburg","SC",1.3092,1.3092]
["45085","Sumter","SC",1.1782,1.1782]
["45087","Union","SC",1.3036,1.3036]
["45089","Williamsburg","SC",1.2646,1.2646]
["45091","York","SC",1.2239,1.2239]
["46003","Aurora","SD",1.3006,1.3006]
["46005","Beadle","SD",0.9669,0.9669]
["46007","Bennett","SD",1.348,1.348]
["46009","Bon Homme","SD",1.24,1.24]
["46011","Brookings","SD",1.2379,1.2379]
["46013","Brown","SD",1.2105,1.2105]
["46015","Brule","SD",1.1139,1.1139]
["46017","Buffalo","SD",0.924,0.924]
["46019","Butte","SD",1.1473,1.1473]
["46021","Campbell","SD",1.0362,1.0362]
["46023","Charles Mix","SD",1.2398,1.2398]
["46025","Clark","SD",1.2717,1.2717]
["46027","Clay","SD",1.2369,1.2369]
["46029","Codington","SD",1.1183,1.1183]
["46031","Corson","SD",1.3006,1.3006]
["46033","Custer","SD",1.294,1.294]
["46035","Davison","SD",1.2022,1.2022]
["46037","Day","SD",1.2609,1.2609]
["46039","Deuel","SD",1.1299,1.1299]
["46041","Dewey","SD",1.2585,1.2585]
["46043","Douglas","SD",1.1577,1.1577]
["46045","Edmunds","SD",1.1299,1.1299]
["46047","Fall River","SD",1.0926,1.0926]
["46049","Faulk","SD",1.3006,1.3006]
["46051","Grant","SD",1.2873,1.2873]
["46053","Gregory","SD",1.3006,1.3006]
["46055","Haakon","SD",1.3006,1.3006]
["46057","Hamlin","SD",0.9974,0.9974]
["46059","Hand","SD",1.1299,1.1299]
["46061","Hanson","SD",1.1942,1.1942]
["46063","Harding","SD",1.3006,1.3006]
["46065","Hughes","SD",1.151,1.151]
["46067","Hutchinson","SD",1.1925,1.1925]
["46069","Hyde","SD",1.24,1.24]
["46071","Jackson","SD",0.9846,0.9846]
["46073","Jerauld","SD",1.1299,1.1299]
["46075","Jones","SD",1.3006,1.3006]
["46077","Kingsbury","SD",1.2612,1.2612]
["46079","Lake","SD",1.1299,1.1299]
["46081","Lawrence","SD",1.0274,1.0274]
["46083","Lincoln","SD",1.2145,1.2145]
["46085","Lyman","SD",1.2322,1.2322]
["46087","McCook","SD",1.0297,1.0297]
["46089","McPherson","SD",1.1299,1.1299]
["46091","Marshall","SD",1.3006,1.3006]
["46093","Meade","SD",1.1826,1.1826]
["46095","Mellette","SD",1.3006,1.3006]
["46097","Miner","SD",1.3006,1.3006]
["46099","Minnehaha","SD",1.1768,1.1768]
["46101","Moody","SD",1.2168,1.2168]
["46102","Oglala Lakota","SD",1.19,1.19]
["46103","Pennington","SD",1.0576,1.0576]
["46105","Perkins","SD",1.031,1.031]
["46107","Potter","SD",1.3044,1.3044]
["46109","Roberts","SD",1.1765,1.1765]
["46111","Sanborn","SD",1.2602,1.2602]
["46115","Spink","SD",1.2383,1.2383]
["46117","Stanley","SD",1.1825,1.1825]
["46119","Sully","SD",1.031,1.031]
["46121","Todd","SD",1.3006,1.3006]
["46123","Tripp","SD",1.3006,1.3006]
["46125","Turner","SD",1.2323,1.2323]
["46127","Union","SD",1.3006,1.3006]
["46129","Walworth","SD",1.3006,1.3006]
["46135","Yankton","SD",1.2398,1.2398]
["46137","Ziebach","SD",1.1328,1.1328]
["47001","Anderson","TN",1.2022,1.2022]
["47003","Bedford","TN",1.2234,1.2234]
["47005","Benton","TN",1.3558,1.3558]
["47007","Bledsoe","TN",1.2436,1.2436]
["47009","Blount","TN",1.2582,1.2582]
["47011","Bradley","TN",1.1733,1.1733]
["47013","Campbell","TN",1.2704,1.2704]
["47015","Cannon","TN",1.2311,1.2311]
["47017","Carroll","TN",1.3811,1.3811]
["47019","Carter","TN",1.1806,1.1806]
["47021","Cheatham","TN",1.4689,1.4689]
["47023","Chester","TN",1.3955,1.3955]
["47025","Claiborne","TN",1.4443,1.4443]
["47027","Clay","TN",1.2337,1.2337]
["47029","Cocke","TN",1.2886,1.2886]
["47031","Coffee","TN",1.2998,1.2998]
["47033","Crockett","TN",1.2022,1.2022]
["47035","Cumberland","TN",1.226,1.226]
["47037","Davidson","TN",1.3331,1.3331]
["47039","Decatur","TN",1.3381,1.3381]
["47041","Dekalb","TN",1.0047,1.0047]
["47043","Dickson","TN",1.3368,1.3368]
["47045","Dyer","TN",1.0076,1.0076]
["47047","Fayette","TN",1.3984,1.3984]
["47049","Fentress","TN",1.3367,1.3367]
["47051","Franklin","TN",1.3296,1.3296]
["47053","Gibson","TN",1.4201,1.4201]
["47055","Giles","TN",1.3154,1.3154]
["47057","Grainger","TN",1.14,1.14]
["47059","Greene","TN",1.2313,1.2313]
["47061","Grundy","TN",1.3492,1.3492]
["47063","Hamblen","TN",1.2022,1.2022]
["47065","Hamilton","TN",1.2694,1.2694]
["47067","Hancock","TN",1.3762,1.3762]
["47069","Hardeman","TN",1.3511,1.3511]
["47071","Hardin","TN",1.2884,1.2884]
["47073","Hawkins","TN",1.4082,1.4082]
["47075","Haywood","TN",1.4357,1.4357]
["47077","Henderson","TN",1.3769,1.3769]
["47079","Henry","TN",1.3208,1.3208]
["47081","Hickman","TN",1.3451,1.3451]
["47083","Houston","TN",1.3576,1.3576]
["47085","Humphreys","TN",1.3823,1.3823]
["47087","Jackson","TN",1.306,1.306]
["47089","Jefferson","TN",1.3114,1.3114]
["47091","Johnson","TN",1.2221,1.2221]
["47093","Knox","TN",1.346,1.346]
["47095","Lake","TN",1.2022,1.2022]
["47097","Lauderdale","TN",1.287,1.287]
["47099","Lawrence","TN",1.2861,1.2861]
["47101","Lewis","TN",1.4255,1.4255]
["47103","Lincoln","TN",1.2283,1.2283]
["47105","Loudon","TN",1.2085,1.2085]
["47107","McMinn","TN",1.2102,1.2102]
["47109","McNairy","TN",1.3239,1.3239]
["47111","Macon","TN",1.1783,1.1783]
["47113","Madison","TN",1.314,1.314]
["47115","Marion","TN",1.3778,1.3778]
["47117","Marshall","TN",1.4251,1.4251]
["47119","Maury","TN",1.2991,1.2991]
["47121","Meigs","TN",1.1366,1.1366]
["47123","Monroe","TN",1.1813,1.1813]
["47125","Montgomery","TN",1.398,1.398]
["47127","Moore","TN",1.4181,1.4181]
["47129","Morgan","TN",1.3106,1.3106]
["47131","Obion","TN",1.2649,1.2649]
["47133","Overton","TN",1.0944,1.0944]
["47135","Perry","TN",1.3683,1.3683]
["47137","Pickett","TN",1.3124,1.3124]
["47139","Polk","TN",1.152,1.152]
["47141","Putnam","TN",1.2913,1.2913]
["47143","Rhea","TN",1.2863,1.2863]
["47145","Roane","TN",1.2111,1.2111]
["47147","Robertson","TN",1.2328,1.2328]
["47149","Rutherford","TN",1.3292,1.3292]
["47151","Scott","TN",1.3051,1.3051]
["47153","Sequatchie","TN",1.2811,1.2811]
["47155","Sevier","TN",1.202,1.202]
["47157","Shelby","TN",1.1731,1.1731]
["47159","Smith","TN",1.1305,1.1305]
["47161","Stewart","TN",1.3499,1.3499]
["47163","Sullivan","TN",1.2132,1.2132]
["47165","Sumner","TN",1.3184,1.3184]
["47167","Tipton","TN",1.1405,1.1405]
["47169","Trousdale","TN",1.348,1.348]
["47171","Unicoi","TN",1.1823,1.1823]
["47173","Union","TN",1.1055,1.1055]
["47175","Van Buren","TN",1.2758,1.2758]
["47177","Warren","TN",1.3668,1.3668]
["47179","Washington","TN",1.2736,1.2736]
["47181","Wayne","TN",1.3328,1.3328]
["47183","Weakley","TN",1.3804,1.3804]
["47185","White","TN",1.3284,1.3284]
["47187","Williamson","TN",1.3371,1.3371]
["47189","Wilson","TN",1.1797,1.1797]
["48001","Anderson","TX",1.2704,1.2704]
["48003","Andrews","TX",1.2906,1.2906]
["48005","Angelina","TX",1.2935,1.2935]
["48007","Aransas","TX",1.2906,1.2906]
["48009","Archer","TX",1.2906,1.2906]
["48011","Armstrong","TX",1.2906,1.2906]
["48013","Atascosa","TX",1.2906,1.2906]
["48015","Austin","TX",1.2906,1.2906]
["48017","Bailey","TX",1.2906,1.2906]
["48019","Bandera","TX",1.2906,1.2906]
["48021","Bastrop","TX",1.2906,1.2906]
["48023","Baylor","TX",1.2906,1.2906]
["48025","Bee","TX",1.2906,1.2906]
["48027","Bell","TX",1.2906,1.2906]
["48029","Bexar","TX",1.2906,1.2906]
["48031","Blanco","TX",1.2906,1.2906]
["48033","Borden","TX",1.2906,1.2906]
["48035","Bosque","TX",1.2906,1.2906]
["48037","Bowie","TX",1.3883,1.3883]
["48039","Brazoria","TX",1.2906,1.2906]
["48041","Brazos","TX",1.2906,1.2906]
["48043","Brewster","TX",1.2906,1.2906]
["48045","Briscoe","TX",1.2906,1.2906]
["48047","Brooks","TX",1.2906,1.2906]
["48049","Brown","TX",1.2906,1.2906]
["48051","Burleson","TX",1.2906,1.2906]
["48053","Burnet","TX",1.2906,1.2906]
["48055","Caldwell","TX",1.2906,1.2906]
["48057","Calhoun","TX",1.2906,1.2906]
["48059","Callahan","TX",1.2906,1.2906]
["48061","Cameron","TX",1.2906,1.2906]
["48063","Camp","TX",1.3845,1.3845]
["48065","Carson","TX",1.2906,1.2906]
["48067","Cass","TX",1.3177,1.3177]
["48069","Castro","TX",1.2906,1.2906]
["48071","Chambers","TX",1.3978,1.3978]
["48073","Cherokee","TX",1.3187,1.3187]
["48075","Childress","TX",1.2906,1.2906]
["48077","Clay","TX",1.2906,1.2906]
["48079","Cochran","TX",1.2906,1.2906]
["48081","Coke","TX",1.2906,1.2906]
["48083","Coleman","TX",1.2906,1.2906]
["48085","Collin","TX",1.2906,1.2906]
["48087","Collingsworth","TX",1.2906,1.2906]
["48089","Colorado","TX",1.2906,1.2906]
["48091","Comal","TX",1.2906,1.2906]
["48093","Comanche","TX",1.2906,1.2906]
["48095","Concho","TX",1.2906,1.2906]
["48097","Cooke","TX",1.2906,1.2906]
["48099","Coryell","TX",1.2906,1.2906]
["48101","Cottle","TX",1.2906,1.2906]
["48103","Crane","TX",1.2906,1.2906]
["48105","Crockett","TX",1.2906,1.2906]
["48107","Crosby","TX",1.2906,1.2906]
["48109","Culberson","TX",1.2906,1.2906]
["48111","Dallam","TX",1.2906,1.2906]
["48113","Dallas","TX",1.2906,1.2906]
["48115","Dawson","TX",1.2906,1.2906]
["48117","Deaf Smith","TX",1.2906,1.2906]
["48119","Delta","TX",1.2906,1.2906]
["48121","Denton","TX",1.2906,1.2906]
["48123","De Witt","TX",1.2906,1.2906]
["48125","Dickens","TX",1.2906,1.2906]
["48127","Dimmit","TX",1.2906,1.2906]
["48129","Donley","TX",1.2906,1.2906]
["48131","Duval","TX",1.2906,1.2906]
["48133","Eastland","TX",1.2906,1.2906]
["48135","Ector","TX",1.2906,1.2906]
["48137","Edwards","TX",1.2906,1.2906]
["48139","Ellis","TX",1.2906,1.2906]
["48141","El Paso","TX",1.2906,1.2906]
["48143","Erath","TX",1.2906,1.2906]
["48145","Falls","TX",1.2906,1.2906]
["48147","Fannin","TX",1.2906,1.2906]
["48149","Fayette","TX",1.2906,1.2906]
["48151","Fisher","TX",1.2906,1.2906]
["48153","Floyd","TX",1.2906,1.2906]
["48155","Foard","TX",1.2906,1.2906]
["48157","Fort Bend","TX",1.2906,1.2906]
["48159","Franklin","TX",1.3332,1.3332]
["48161","Freestone","TX",1.2906,1.2906]
["48163","Frio","TX",1.2906,1.2906]
["48165","Gaines","TX",1.2906,1.2906]
["48167","Galveston","TX",1.2906,1.2906]
["48169","Garza","TX",1.2906,1.2906]
["48171","Gillespie","TX",1.2906,1.2906]
["48173","Glasscock","TX",1.2906,1.2906]
["48175","Goliad","TX",1.2906,1.2906]
["48177","Gonzales","TX",1.2906,1.2906]
["48179","Gray","TX",1.2906,1.2906]
["48181","Grayson","TX",1.2906,1.2906]
["48183","Gregg","TX",1.4035,1.4035]
["48185","Grimes","TX",1.1808,1.1808]
["48187","Guadalupe","TX",1.2906,1.2906]
["48189","Hale","TX",1.2906,1.2906]
["48191","Hall","TX",1.2906,1.2906]
["48193","Hamilton","TX",1.2906,1.2906]
["48195","Hansford","TX",1.2906,1.2906]
["48197","Hardeman","TX",1.2906,1.2906]
["48199","Hardin","TX",1.371,1.371]
["48201","Harris","TX",1.2996,1.2996]
["48203","Harrison","TX",1.3253,1.3253]
["48205","Hartley","TX",1.2906,1.2906]
["48207","Haskell","TX",1.2906,1.2906]
["48209","Hays","TX",1.2906,1.2906]
["48211","Hemphill","TX",1.2906,1.2906]
["48213","Henderson","TX",1.3794,1.3794]
["48215","Hidalgo","TX",1.2906,1.2906]
["48217","Hill","TX",1.2906,1.2906]
["48219","Hockley","TX",1.2906,1.2906]
["48221","Hood","TX",1.2906,1.2906]
["48223","Hopkins","TX",1.2906,1.2906]
["48225","Houston","TX",1.3093,1.3093]
["48227","Howard","TX",1.2906,1.2906]
["48229","Hudspeth","TX",1.2906,1.2906]
["48231","Hunt","TX",1.2906,1.2906]
["48233","Hutchinson","TX",1.2906,1.2906]
["48235","Irion","TX",1.2906,1.2906]
["48237","Jack","TX",1.2906,1.2906]
["48239","Jackson","TX",1.2906,1.2906]
["48241","Jasper","TX",1.357,1.357]
["48243","Jeff Davis","TX",1.2906,1.2906]
["48245","Jefferson","TX",1.4055,1.4055]
["48247","Jim Hogg","TX",1.2906,1.2906]
["48249","Jim Wells","TX",1.2906,1.2906]
["48251","Johnson","TX",1.2906,1.2906]
["48253","Jones","TX",1.2906,1.2906]
["48255","Karnes","TX",1.2906,1.2906]
["48257","Kaufman","TX",1.2906,1.2906]
["48259","Kendall","TX",1.2906,1.2906]
["48261","Kenedy","TX",1.2906,1.2906]
["48263","Kent","TX",1.2906,1.2906]
["48265","Kerr","TX",1.2906,1.2906]
["48267","Kimble","TX",1.2906,1.2906]
["48269","King","TX",1.2906,1.2906]
["48271","Kinney","TX",1.2906,1.2906]
["48273","Kleberg","TX",1.2906,1.2906]
["48275","Knox","TX",1.2906,1.2906]
["48277","Lamar","TX",1.2906,1.2906]
["48279","Lamb","TX",1.2906,1.2906]
["48281","Lampasas","TX",1.2906,1.2906]
["48283","La Salle","TX",1.2906,1.2906]
["48285","Lavaca","TX",1.2906,1.2906]
["48287","Lee","TX",1.2906,1.2906]
["48289","Leon","TX",1.4046,1.4046]
["48291","Liberty","TX",1.2973,1.2973]
["48293","Limestone","TX",1.2906,1.2906]
["48295","Lipscomb","TX",1.2906,1.2906]
["48297","Live Oak","TX",1.2906,1.2906]
["48299","Llano","TX",1.2906,1.2906]
["48301","Loving","TX",1.2906,1.2906]
["48303","Lubbock","TX",1.2906,1.2906]
["48305","Lynn","TX",1.2906,1.2906]
["48307","McCulloch","TX",1.2906,1.2906]
["48309","McLennan","TX",1.2906,1.2906]
["48311","McMullen","TX",1.2906,1.2906]
["48313","Madison","TX",1.2755,1.2755]
["48315","Marion","TX",1.3008,1.3008]
["48317","Martin","TX",1.2906,1.2906]
["48319","Mason","TX",1.2906,1.2906]
["48321","Matagorda","TX",1.2906,1.2906]
["48323","Maverick","TX",1.2906,1.2906]
["48325","Medina","TX",1.2906,1.2906]
["48327","Menard","TX",1.2906,1.2906]
["48329","Midland","TX",1.2906,1.2906]
["48331","Milam","TX",1.2906,1.2906]
["48333","Mills","TX",1.2906,1.2906]
["48335","Mitchell","TX",1.2906,1.2906]
["48337","Montague","TX",1.2906,1.2906]
["48339","Montgomery","TX",1.2875,1.2875]
["48341","Moore","TX",1.2906,1.2906]
["48343","Morris","TX",1.3951,1.3951]
["48345","Motley","TX",1.2906,1.2906]
["48347","Nacogdoches","TX",1.2928,1.2928]
["48349","Navarro","TX",1.2906,1.2906]
["48351","Newton","TX",1.3476,1.3476]
["48353","Nolan","TX",1.2906,1.2906]
["48355","Nueces","TX",1.2906,1.2906]
["48357","Ochiltree","TX",1.2906,1.2906]
["48359","Oldham","TX",1.2906,1.2906]
["48361","Orange","TX",1.3574,1.3574]
["48363","Palo Pinto","TX",1.2906,1.2906]
["48365","Panola","TX",1.3527,1.3527]
["48367","Parker","TX",1.2906,1.2906]
["48369","Parmer","TX",1.2906,1.2906]
["48371","Pecos","TX",1.2906,1.2906]
["48373","Polk","TX",1.2855,1.2855]
["48375","Potter","TX",1.2906,1.2906]
["48377","Presidio","TX",1.2906,1.2906]
["48379","Rains","TX",1.2906,1.2906]
["48381","Randall","TX",1.2906,1.2906]
["48383","Reagan","TX",1.2906,1.2906]
["48385","Real","TX",1.2906,1.2906]
["48387","Red River","TX",1.4167,1.4167]
["48389","Reeves","TX",1.2906,1.2906]
["48391","Refugio","TX",1.2906,1.2906]
["48393","Roberts","TX",1.2906,1.2906]
["48395","Robertson","TX",1.2906,1.2906]
["48397","Rockwall","TX",1.2906,1.2906]
["48399","Runnels","TX",1.2906,1.2906]
["48401","Rusk","TX",1.3859,1.3859]
["48403","Sabine","TX",1.3439,1.3439]
["48405","San Augustine","TX",1.3245,1.3245]
["48407","San Jacinto","TX",1.297,1.297]
["48409","San Patricio","TX",1.2906,1.2906]
["48411","San Saba","TX",1.2906,1.2906]
["48413","Schleicher","TX",1.2906,1.2906]
["48415","Scurry","TX",1.2906,1.2906]
["48417","Shackelford","TX",1.2906,1.2906]
["48419","Shelby","TX",1.3062,1.3062]
["48421","Sherman","TX",1.2906,1.2906]
["48423","Smith","TX",1.3208,1.3208]
["48425","Somervell","TX",1.2906,1.2906]
["48427","Starr","TX",1.2906,1.2906]
["48429","Stephens","TX",1.2906,1.2906]
["48431","Sterling","TX",1.2906,1.2906]
["48433","Stonewall","TX",1.2906,1.2906]
["48435","Sutton","TX",1.2906,1.2906]
["48437","Swisher","TX",1.2906,1.2906]
["48439","Tarrant","TX",1.2906,1.2906]
["48441","Taylor","TX",1.2906,1.2906]
["48443","Terrell","TX",1.2906,1.2906]
["48445","Terry","TX",1.2906,1.2906]
["48447","Throckmorton","TX",1.2906,1.2906]
["48449","Titus","TX",1.3883,1.3883]
["48451","Tom Green","TX",1.2906,1.2906]
["48453","Travis","TX",1.2906,1.2906]
["48455","Trinity","TX",1.3302,1.3302]
["48457","Tyler","TX",1.3226,1.3226]
["48459","Upshur","TX",1.4212,1.4212]
["48461","Upton","TX",1.2906,1.2906]
["48463","Uvalde","TX",1.2906,1.2906]
["48465","Val Verde","TX",1.2906,1.2906]
["48467","Van Zandt","TX",1.4134,1.4134]
["48469","Victoria","TX",1.2906,1.2906]
["48471","Walker","TX",1.281,1.281]
["48473","Waller","TX",1.2906,1.2906]
["48475","Ward","TX",1.2906,1.2906]
["48477","Washington","TX",1.2906,1.2906]
["48479","Webb","TX",1.2906,1.2906]
["48481","Wharton","TX",1.2906,1.2906]
["48483","Wheeler","TX",1.2906,1.2906]
["48485","Wichita","TX",1.2906,1.2906]
["48487","Wilbarger","TX",1.2906,1.2906]
["48489","Willacy","TX",1.2906,1.2906]
["48491","Williamson","TX",1.2906,1.2906]
["48493","Wilson","TX",1.2906,1.2906]
["48495","Winkler","TX",1.2906,1.2906]
["48497","Wise","TX",1.2906,1.2906]
["48499","Wood","TX",1.38,1.38]
["48501","Yoakum","TX",1.2906,1.2906]
["48503","Young","TX",1.2906,1.2906]
["48505","Zapata","TX",1.2906,1.2906]
["48507","Zavala","TX",1.2906,1.2906]
["49001","Beaver","UT",1.0259,1.0259]
["49003","Box Elder","UT",1.017,1.017]
["49005","Cache","UT",1.017,1.017]
["49007","Carbon","UT",1.0177,1.0177]
["49009","Daggett","UT",1.017,1.017]
["49011","Davis","UT",1.0992,1.0992]
["49013","Duchesne","UT",1.0533,1.0533]
["49015","Emery","UT",1.0177,1.0177]
["49017","Garfield","UT",1.0541,1.0541]
["49019","Grand","UT",1.0177,1.0177]
["49021","Iron","UT",1.0171,1.0171]
["49023","Juab","UT",1.0276,1.0276]
["49025","Kane","UT",1.0554,1.0554]
["49027","Millard","UT",1.0259,1.0259]
["49029","Morgan","UT",1.017,1.017]
["49031","Piute","UT",1.0529,1.0529]
["49033","Rich","UT",1.0567,1.0567]
["49035","Salt Lake","UT",1.017,1.017]
["49037","San Juan","UT",1.0276,1.0276]
["49039","Sanpete","UT",1.056,1.056]
["49041","Sevier","UT",1.0522,1.0522]
["49043","Summit","UT",1.0539,1.0539]
["49045","Tooele","UT",1.0276,1.0276]
["49047","Uintah","UT",1.0576,1.0576]
["49049","Utah","UT",1.0308,1.0308]
["49051","Wasatch","UT",1.0542,1.0542]
["49053","Washington","UT",1.0171,1.0171]
["49055","Wayne","UT",1.0198,1.0198]
["49057","Weber","UT",1.0276,1.0276]
["50001","Addison","VT",1.3635,1.3635]
["50003","Bennington","VT",1.3053,1.3053]
["50005","Caledonia","VT",1.2598,1.2598]
["50007","Chittenden","VT",1.3425,1.3425]
["50009","Essex","VT",1.2261,1.2261]
["50011","Franklin","VT",1.2942,1.2942]
["50013","Grand Isle","VT",1.2934,1.2934]
["50015","Lamoille","VT",1.3144,1.3144]
["50017","Orange","VT",1.3366,1.3366]
["50019","Orleans","VT",1.279,1.279]
["50021","Rutland","VT",1.3277,1.3277]
["50023","Washington","VT",1.3207,1.3207]
["50025","Windham","VT",1.3183,1.3183]
["50027","Windsor","VT",1.3111,1.3111]
["51001","Accomack","VA",1.2278,1.2278]
["51003","Albemarle","VA",1.158,1.158]
["51005","Alleghany","VA",1.304,1.304]
["51007","Amelia","VA",1.293,1.293]
["51009","Amherst","VA",1.3142,1.3142]
["51011","Appomattox","VA",1.3767,1.3767]
["51013","Arlington","VA",1.2906,1.2906]
["51015","Augusta","VA",1.3983,1.3983]
["51017","Bath","VA",1.334,1.334]
["51019","Bedford","VA",1.2347,1.2347]
["51021","Bland","VA",1.1828,1.1828]
["51023","Botetourt","VA",1.256,1.256]
["51025","Brunswick","VA",1.209,1.209]
["51027","Buchanan","VA",1.2277,1.2277]
["51029","Buckingham","VA",1.2931,1.2931]
["51031","Campbell","VA",1.3247,1.3247]
["51033","Caroline","VA",1.3295,1.3295]
["51035","Carroll","VA",1.3792,1.3792]
["51036","Charles City","VA",1.2773,1.2773]
["51037","Charlotte","VA",1.0896,1.0896]
["51041","Chesterfield","VA",1.3313,1.3313]
["51043","Clarke","VA",1.2022,1.2022]
["51045","Craig","VA",1.3892,1.3892]
["51047","Culpeper","VA",1.2744,1.2744]
["51049","Cumberland","VA",1.1967,1.1967]
["51051","Dickenson","VA",1.3139,1.3139]
["51053","Dinwiddie","VA",1.2884,1.2884]
["51057","Essex","VA",1.2771,1.2771]
["51059","Fairfax","VA",1.2761,1.2761]
["51061","Fauquier","VA",1.3776,1.3776]
["51063","Floyd","VA",1.1814,1.1814]
["51065","Fluvanna","VA",1.3247,1.3247]
["51067","Franklin","VA",1.2657,1.2657]
["51069","Frederick","VA",1.4196,1.4196]
["51071","Giles","VA",1.3587,1.3587]
["51073","Gloucester","VA",1.2045,1.2045]
["51075","Goochland","VA",1.2814,1.2814]
["51077","Grayson","VA",1.3067,1.3067]
["51079","Greene","VA",1.2015,1.2015]
["51081","Greensville","VA",1.2871,1.2871]
["51083","Halifax","VA",1.2018,1.2018]
["51085","Hanover","VA",1.1623,1.1623]
["51087","Henrico","VA",1.2669,1.2669]
["51089","Henry","VA",1.1467,1.1467]
["51091","Highland","VA",1.3315,1.3315]
["51093","Isle of Wight","VA",1.206,1.206]
["51095","James City","VA",1.1636,1.1636]
["51097","King and Queen","VA",1.2211,1.2211]
["51099","King George","VA",1.1819,1.1819]
["51101","King William","VA",1.2269,1.2269]
["51103","Lancaster","VA",1.2246,1.2246]
["51105","Lee","VA",1.1933,1.1933]
["51107","Loudoun","VA",1.2893,1.2893]
["51109","Louisa","VA",1.3843,1.3843]
["51111","Lunenburg","VA",1.2364,1.2364]
["51113","Madison","VA",1.4096,1.4096]
["51115","Mathews","VA",1.3373,1.3373]
["51117","Mecklenburg","VA",1.3146,1.3146]
["51119","Middlesex","VA",1.0703,1.0703]
["51121","Montgomery","VA",1.3892,1.3892]
["51125","Nelson","VA",1.2503,1.2503]
["51127","New Kent","VA",1.2389,1.2389]
["51131","Northampton","VA",1.2622,1.2622]
["51133","Northumberland","VA",1.3113,1.3113]
["51135","Nottoway","VA",1.3954,1.3954]
["51137","Orange","VA",1.3232,1.3232]
["51139","Page","VA",1.2022,1.2022]
["51141","Patrick","VA",1.1681,1.1681]
["51143","Pittsylvania","VA",1.2138,1.2138]
["51145","Powhatan","VA",1.3611,1.3611]
["51147","Prince Edward","VA",1.2538,1.2538]
["51149","Prince George","VA",1.3165,1.3165]
["51153","Prince William","VA",1.3554,1.3554]
["51155","Pulaski","VA",1.2022,1.2022]
["51157","Rappahannock","VA",1.402,1.402]
["51159","Richmond","VA",1.2854,1.2854]
["51161","Roanoke","VA",1.3422,1.3422]
["51163","Rockbridge","VA",1.3497,1.3497]
["51165","Rockingham","VA",1.377,1.377]
["51167","Russell","VA",1.4108,1.4108]
["51169","Scott","VA",1.1986,1.1986]
["51171","Shenandoah","VA",1.4936,1.4936]
["51173","Smyth","VA",1.3582,1.3582]
["51175","Southampton","VA",1.2622,1.2622]
["51177","Spotsylvania","VA",1.1832,1.1832]
["51179","Stafford","VA",1.0814,1.0814]
["51181","Surry","VA",1.3135,1.3135]
["51183","Sussex","VA",1.264,1.264]
["51185","Tazewell","VA",1.3116,1.3116]
["51187","Warren","VA",1.3584,1.3584]
["51191","Washington","VA",1.3462,1.3462]
["51193","Westmoreland","VA",1.2904,1.2904]
["51195","Wise","VA",1.2917,1.2917]
["51197","Wythe","VA",1.4545,1.4545]
["51199","York","VA",1.5347,1.5347]
["51510","Alexandria City","VA",1.2906,1.2906]
["51520","Bristol City","VA",1.2906,1.2906]
["51530","Buena Vista City","VA",1.2906,1.2906]
["51540","Charlottesville City","VA",1.2906,1.2906]
["51550","Chesapeake City","VA",1.181,1.181]
["51570","Colonial Heights City","VA",1.2906,1.2906]
["51580","Covington City","VA",1.2906,1.2906]
["51590","Danville City","VA",1.2906,1.2906]
["51595","Emporia City","VA",1.2906,1.2906]
["51600","Fairfax City","VA",1.2906,1.2906]
["51610","Falls Church City","VA",1.2906,1.2906]
["51620","Franklin City","VA",1.2906,1.2906]
["51630","Fredericksburg City","VA",1.2906,1.2906]
["51640","Galax City","VA",1.2906,1.2906]
["51650","Hampton City","VA",1.2557,1.2557]
["51660","Harrisonburg City","VA",1.2906,1.2906]
["51670","Hopewell City","VA",1.2906,1.2906]
["51678","Lexington City","VA",1.2906,1.2906]
["51680","Lynchburg City","VA",1.2906,1.2906]
["51683","Manassas City","VA",1.2906,1.2906]
["51685","Manassas Park City","VA",1.2906,1.2906]
["51690","Martinsville City","VA",1.2906,1.2906]
["51700","Newport News City","VA",1.3602,1.3602]
["51710","Norfolk City","VA",1.2906,1.2906]
["51720","Norton City","VA",1.2906,1.2906]
["51730","Petersburg City","VA",1.2906,1.2906]
["51735","Poquoson City","VA",1.2906,1.2906]
["51740","Portsmouth City","VA",1.2906,1.2906]
["51750","Radford","VA",1.2906,1.2906]
["51760","Richmond City","VA",1.2906,1.2906]
["51770","Roanoke City","VA",1.2906,1.2906]
["51775","Salem City","VA",1.2906,1.2906]
["51790","Staunton City","VA",1.2906,1.2906]
["51800","Suffolk City","VA",1.1896,1.1896]
["51810","Virginia Beach City","VA",1.1558,1.1558]
["51820","Waynesboro City","VA",1.2906,1.2906]
["51830","Williamsburg City","VA",1.2906,1.2906]
["51840","Winchester City","VA",1.2906,1.2906]
["53001","Adams","WA",1.0276,1.0276]
["53003","Asotin","WA",1.0276,1.0276]
["53005","Benton","WA",1.0276,1.0276]
["53007","Chelan","WA",1.017,1.017]
["53009","Clallam","WA",1.028,1.028]
["53011","Clark","WA",1.0276,1.0276]
["53013","Columbia","WA",1.0276,1.0276]
["53015","Cowlitz","WA",1.028,1.028]
["53017","Douglas","WA",1.0276,1.0276]
["53019","Ferry","WA",1.017,1.017]
["53021","Franklin","WA",1.0276,1.0276]
["53023","Garfield","WA",1.0276,1.0276]
["53025","Grant","WA",1.0276,1.0276]
["53027","Grays Harbor","WA",1.0281,1.0281]
["53029","Island","WA",1.0276,1.0276]
["53031","Jefferson","WA",1.017,1.017]
["53033","King","WA",1.017,1.017]
["53035","Kitsap","WA",1.0276,1.0276]
["53037","Kittitas","WA",1.017,1.017]
["53039","Klickitat","WA",1.017,1.017]
["53041","Lewis","WA",1.028,1.028]
["53043","Lincoln","WA",1.0276,1.0276]
["53045","Mason","WA",1.028,1.028]
["53047","Okanogan","WA",1.017,1.017]
["53049","Pacific","WA",1.0281,1.0281]
["53051","Pend Oreille","WA",1.017,1.017]
["53053","Pierce","WA",1.0281,1.0281]
["53055","San Juan","WA",1.0276,1.0276]
["53057","Skagit","WA",1.0275,1.0275]
["53059","Skamania","WA",1.0276,1.0276]
["53061","Snohomish","WA",1.017,1.017]
["53063","Spokane","WA",1.0276,1.0276]
["53065","Stevens","WA",1.0276,1.0276]
["53067","Thurston","WA",1.0276,1.0276]
["53069","Wahkiakum","WA",1.0276,1.0276]
["53071","Walla Walla","WA",1.0276,1.0276]
["53073","Whatcom","WA",1.017,1.017]
["53075","Whitman","WA",1.0276,1.0276]
["53077","Yakima","WA",1.0279,1.0279]
["54001","Barbour","WV",1.2275,1.2275]
["54003","Berkeley","WV",1.2633,1.2633]
["54005","Boone","WV",1.2689,1.2689]
["54007","Braxton","WV",1.2761,1.2761]
["54009","Brooke","WV",1.2577,1.2577]
["54011","Cabell","WV",1.3004,1.3004]
["54013","Calhoun","WV",1.315,1.315]
["54015","Clay","WV",1.3036,1.3036]
["54017","Doddridge","WV",1.3189,1.3189]
["54019","Fayette","WV",1.2693,1.2693]
["54021","Gilmer","WV",1.3232,1.3232]
["54023","Grant","WV",1.3119,1.3119]
["54025","Greenbrier","WV",1.2623,1.2623]
["54027","Hampshire","WV",1.2003,1.2003]
["54029","Hancock","WV",1.2577,1.2577]
["54031","Hardy","WV",1.2654,1.2654]
["54033","Harrison","WV",1.2662,1.2662]
["54035","Jackson","WV",1.1855,1.1855]
["54037","Jefferson","WV",1.3161,1.3161]
["54039","Kanawha","WV",1.2284,1.2284]
["54041","Lewis","WV",1.2668,1.2668]
["54043","Lincoln","WV",1.2723,1.2723]
["54045","Logan","WV",1.2813,1.2813]
["54047","McDowell","WV",1.2763,1.2763]
["54049","Marion","WV",1.2165,1.2165]
["54051","Marshall","WV",1.2614,1.2614]
["54053","Mason","WV",1.2464,1.2464]
["54055","Mercer","WV",1.2746,1.2746]
["54057","Mineral","WV",1.2447,1.2447]
["54059","Mingo","WV",1.2399,1.2399]
["54061","Monongalia","WV",1.274,1.274]
["54063","Monroe","WV",1.2586,1.2586]
["54065","Morgan","WV",1.2732,1.2732]
["54067","Nicholas","WV",1.243,1.243]
["54069","Ohio","WV",1.2577,1.2577]
["54071","Pendleton","WV",1.2196,1.2196]
["54073","Pleasants","WV",1.254,1.254]
["54075","Pocahontas","WV",1.2435,1.2435]
["54077","Preston","WV",1.259,1.259]
["54079","Putnam","WV",1.1523,1.1523]
["54081","Raleigh","WV",1.2525,1.2525]
["54083","Randolph","WV",1.2663,1.2663]
["54085","Ritchie","WV",1.2853,1.2853]
["54087","Roane","WV",1.2755,1.2755]
["54089","Summers","WV",1.2768,1.2768]
["54091","Taylor","WV",1.2515,1.2515]
["54093","Tucker","WV",1.2032,1.2032]
["54095","Tyler","WV",1.2793,1.2793]
["54097","Upshur","WV",1.2616,1.2616]
["54099","Wayne","WV",1.3116,1.3116]
["54101","Webster","WV",1.2331,1.2331]
["54103","Wetzel","WV",1.2657,1.2657]
["54105","Wirt","WV",1.1876,1.1876]
["54107","Wood","WV",1.1516,1.1516]
["54109","Wyoming","WV",1.2696,1.2696]
["55001","Adams","WI",1.4186,1.4186]
["55003","Ashland","WI",1.3164,1.3164]
["55005","Barron","WI",1.2953,1.2953]
["55007","Bayfield","WI",1.2327,1.2327]
["55009","Brown","WI",1.3357,1.3357]
["55011","Buffalo","WI",1.3031,1.3031]
["55013","Burnett","WI",1.27,1.27]
["55015","Calumet","WI",1.3041,1.3041]
["55017","Chippewa","WI",1.431,1.431]
["55019","Clark","WI",1.2877,1.2877]
["55021","Columbia","WI",1.3555,1.3555]
["55023","Crawford","WI",1.365,1.365]
["55025","Dane","WI",1.3006,1.3006]
["55027","Dodge","WI",1.2499,1.2499]
["55029","Door","WI",1.1489,1.1489]
["55031","Douglas","WI",1.343,1.343]
["55033","Dunn","WI",1.381,1.381]
["55035","Eau Claire","WI",1.4107,1.4107]
["55037","Florence","WI",1.3389,1.3389]
["55039","Fond Du Lac","WI",1.2154,1.2154]
["55041","Forest","WI",1.3463,1.3463]
["55043","Grant","WI",1.3483,1.3483]
["55045","Green","WI",1.3502,1.3502]
["55047","Green Lake","WI",1.0967,1.0967]
["55049","Iowa","WI",1.3006,1.3006]
["55051","Iron","WI",1.3314,1.3314]
["55053","Jackson","WI",1.1766,1.1766]
["55055","Jefferson","WI",1.3706,1.3706]
["55057","Juneau","WI",1.383,1.383]
["55059","Kenosha","WI",1.395,1.395]
["55061","Kewaunee","WI",1.2666,1.2666]
["55063","La Crosse","WI",1.1574,1.1574]
["55065","Lafayette","WI",1.3006,1.3006]
["55067","Langlade","WI",1.3264,1.3264]
["55069","Lincoln","WI",1.2645,1.2645]
["55071","Manitowoc","WI",1.2704,1.2704]
["55073","Marathon","WI",1.3451,1.3451]
["55075","Marinette","WI",1.3657,1.3657]
["55077","Marquette","WI",1.4472,1.4472]
["55078","Menominee","WI",1.478,1.478]
["55079","Milwaukee","WI",1.3134,1.3134]
["55081","Monroe","WI",1.437,1.437]
["55083","Oconto","WI",1.3525,1.3525]
["55085","Oneida","WI",1.3377,1.3377]
["55087","Outagamie","WI",1.3641,1.3641]
["55089","Ozaukee","WI",1.3267,1.3267]
["55091","Pepin","WI",1.3006,1.3006]
["55093","Pierce","WI",1.3006,1.3006]
["55095","Polk","WI",1.3241,1.3241]
["55097","Portage","WI",1.3273,1.3273]
["55099","Price","WI",1.3462,1.3462]
["55101","Racine","WI",1.3475,1.3475]
["55103","Richland","WI",1.333,1.333]
["55105","Rock","WI",1.3543,1.3543]
["55107","Rusk","WI",1.3539,1.3539]
["55109","St Croix","WI",1.3811,1.3811]
["55111","Sauk","WI",1.3006,1.3006]
["55113","Sawyer","WI",1.2739,1.2739]
["55115","Shawano","WI",1.3894,1.3894]
["55117","Sheboygan","WI",1.3372,1.3372]
["55119","Taylor","WI",1.2896,1.2896]
["55121","Trempealeau","WI",1.369,1.369]
["55123","Vernon","WI",1.3006,1.3006]
["55125","Vilas","WI",1.1917,1.1917]
["55127","Walworth","WI",1.4096,1.4096]
["55129","Washburn","WI",1.3126,1.3126]
["55131","Washington","WI",1.357,1.357]
["55133","Waukesha","WI",1.2369,1.2369]
["55135","Waupaca","WI",1.2787,1.2787]
["55137","Waushara","WI",1.4048,1.4048]
["55139","Winnebago","WI",1.2726,1.2726]
["55141","Wood","WI",1.3006,1.3006]
["56001","Albany","WY",1.017,1.017]
["56003","Big Horn","WY",1.0717,1.0717]
["56005","Campbell","WY",1.0276,1.0276]
["56007","Carbon","WY",1.0276,1.0276]
["56009","Converse","WY",1.017,1.017]
["56011","Crook","WY",1.0225,1.0225]
["56013","Fremont","WY",1.017,1.017]
["56015","Goshen","WY",1.0276,1.0276]
["56017","Hot Springs","WY",1.017,1.017]
["56019","Johnson","WY",1.0658,1.0658]
["56021","Laramie","WY",1.0276,1.0276]
["56023","Lincoln","WY",1.0191,1.0191]
["56025","Natrona","WY",1.017,1.017]
["56027","Niobrara","WY",1.0276,1.0276]
["56029","Park","WY",1.0228,1.0228]
["56031","Platte","WY",1.0276,1.0276]
["56033","Sheridan","WY",1.017,1.017]
["56035","Sublette","WY",1.018,1.018]
["56037","Sweetwater","WY",1.0276,1.0276]
["56039","Teton","WY",1.017,1.017]
["56041","Uinta","WY",1.0101,1.0101]
["56043","Washakie","WY",1.0276,1.0276]
["56045","Weston","WY",1.017,1.017]

{"sheet":"cordwood-burnrate","index":7,"n_rows":3147,"n_cols":7,"rows_kept":3147}
[]
[]
["Average of Burn Rate - CORDS WOOD PER APPLIANCE PER COUNTY",null,null,"Appliance Type"]
["StateAndCountyFIPSCode","CountyName","PostalStateCode","Fireplace: general","Furnace","Hydronic heater","Woodstove or Fireplace Insert"]
["01001","Autauga","AL",{"v":0.18850001099999997,"d":"0.19"},{"v":1.1894614125778198,"d":"1.19"},{"v":1.18946141257782,"d":"1.19"},{"v":0.5371707555,"d":"0.54"}]
["01003","Baldwin","AL",{"v":0.19065285800000004,"d":"0.19"},{"v":1.1469591519366562,"d":"1.15"},{"v":1.1469591519366564,"d":"1.15"},{"v":0.48328448,"d":"0.48"}]
["01005","Barbour","AL",{"v":0.20270349400000004,"d":"0.20"},{"v":1.2017041833370596,"d":"1.20"},{"v":1.2017041833370596,"d":"1.20"},{"v":0.5805668064999999,"d":"0.58"}]
["01007","Bibb","AL",{"v":0.199947654,"d":"0.20"},{"v":1.253218759587123,"d":"1.25"},{"v":1.253218759587123,"d":"1.25"},{"v":0.6331551674999999,"d":"0.63"}]
["01009","Blount","AL",{"v":0.21538187500000003,"d":"0.22"},{"v":1.2785294934855878,"d":"1.28"},{"v":1.2785294934855882,"d":"1.28"},{"v":0.5726780079999999,"d":"0.57"}]
["01011","Bullock","AL",{"v":0.197845035,"d":"0.20"},{"v":1.2202044436403412,"d":"1.22"},{"v":1.2202044436403414,"d":"1.22"},{"v":0.5812329345,"d":"0.58"}]
["01013","Butler","AL",{"v":0.20438301400000003,"d":"0.20"},{"v":1.1802182271295074,"d":"1.18"},{"v":1.1802182271295074,"d":"1.18"},{"v":0.615374051,"d":"0.62"}]
["01015","Calhoun","AL",{"v":0.176752271,"d":"0.18"},{"v":1.1809111176300884,"d":"1.18"},{"v":1.1809111176300884,"d":"1.18"},{"v":0.5467005355,"d":"0.55"}]
["01017","Chambers","AL",{"v":0.18947575700000002,"d":"0.19"},{"v":1.2097562853172528,"d":"1.21"},{"v":1.2097562853172528,"d":"1.21"},{"v":0.583303774,"d":"0.58"}]
["01019","Cherokee","AL",{"v":0.217995635,"d":"0.22"},{"v":1.2580785501894978,"d":"1.26"},{"v":1.2580785501894978,"d":"1.26"},{"v":0.552219407,"d":"0.55"}]
["01021","Chilton","AL",{"v":0.21128675900000002,"d":"0.21"},{"v":1.2683132583392498,"d":"1.27"},{"v":1.2683132583392498,"d":"1.27"},{"v":0.5910466235,"d":"0.59"}]
["01023","Choctaw","AL",{"v":0.216453985,"d":"0.22"},{"v":1.24286281940821,"d":"1.24"},{"v":1.2428628194082099,"d":"1.24"},{"v":0.653061538,"d":"0.65"}]
["01025","Clarke","AL",{"v":0.20412908399999996,"d":"0.20"},{"v":1.184197272538976,"d":"1.18"},{"v":1.184197272538976,"d":"1.18"},{"v":0.6304384865,"d":"0.63"}]
["01027","Clay","AL",{"v":0.21644249300000007,"d":"0.22"},{"v":1.2056084951117905,"d":"1.21"},{"v":1.2056084951117905,"d":"1.21"},{"v":0.655368155,"d":"0.66"}]
["01029","Cleburne","AL",{"v":0.214837534,"d":"0.21"},{"v":1.2685674263922118,"d":"1.27"},{"v":1.2685674263922118,"d":"1.27"},{"v":0.6516981375,"d":"0.65"}]
["01031","Coffee","AL",{"v":0.203473563,"d":"0.20"},{"v":1.1877856709276504,"d":"1.19"},{"v":1.1877856709276504,"d":"1.19"},{"v":0.5289139305,"d":"0.53"}]
["01033","Colbert","AL",{"v":0.194529415,"d":"0.19"},{"v":1.2087539842739343,"d":"1.21"},{"v":1.2087539842739345,"d":"1.21"},{"v":0.517256117,"d":"0.52"}]
["01035","Conecuh","AL",{"v":0.215983524,"d":"0.22"},{"v":1.1984814519671896,"d":"1.20"},{"v":1.1984814519671896,"d":"1.20"},{"v":0.6048395110000001,"d":"0.60"}]
["01037","Coosa","AL",{"v":0.216151372,"d":"0.22"},{"v":1.267145952112865,"d":"1.27"},{"v":1.2671459521128652,"d":"1.27"},{"v":0.6502540645,"d":"0.65"}]
["01039","Covington","AL",{"v":0.20987318599999996,"d":"0.21"},{"v":1.1719016467606373,"d":"1.17"},{"v":1.1719016467606371,"d":"1.17"},{"v":0.5721796090000001,"d":"0.57"}]
["01041","Crenshaw","AL",{"v":0.22236417700000002,"d":"0.22"},{"v":1.17361047890497,"d":"1.17"},{"v":1.17361047890497,"d":"1.17"},{"v":0.617449703,"d":"0.62"}]
["01043","Cullman","AL",{"v":0.205831198,"d":"0.21"},{"v":1.2663625886605283,"d":"1.27"},{"v":1.2663625886605283,"d":"1.27"},{"v":0.534520108,"d":"0.53"}]
["01045","Dale","AL",{"v":0.20363010899999998,"d":"0.20"},{"v":1.18563979059875,"d":"1.19"},{"v":1.18563979059875,"d":"1.19"},{"v":0.540116682,"d":"0.54"}]
["01047","Dallas","AL",{"v":0.199510467,"d":"0.20"},{"v":1.1081782852431623,"d":"1.11"},{"v":1.1081782852431625,"d":"1.11"},{"v":0.548742045,"d":"0.55"}]
["01049","De Kalb","AL",{"v":0.219736376,"d":"0.22"},{"v":1.271606515036984,"d":"1.27"},{"v":1.271606515036984,"d":"1.27"},{"v":0.547036314,"d":"0.55"}]
["01051","Elmore","AL",{"v":0.19680967000000002,"d":"0.20"},{"v":1.2213505494022507,"d":"1.22"},{"v":1.2213505494022507,"d":"1.22"},{"v":0.5502185685000001,"d":"0.55"}]
["01053","Escambia","AL",{"v":0.206333994,"d":"0.21"},{"v":1.1784660120964099,"d":"1.18"},{"v":1.1784660120964097,"d":"1.18"},{"v":0.555233367,"d":"0.56"}]
["01055","Etowah","AL",{"v":0.182605929,"d":"0.18"},{"v":1.1538300500390775,"d":"1.15"},{"v":1.1538300500390775,"d":"1.15"},{"v":0.5190949525,"d":"0.52"}]
["01057","Fayette","AL",{"v":0.206645073,"d":"0.21"},{"v":1.2293965367200823,"d":"1.23"},{"v":1.229396536720082,"d":"1.23"},{"v":0.6417560255,"d":"0.64"}]
["01059","Franklin","AL",{"v":0.20282323900000002,"d":"0.20"},{"v":1.2150759303803387,"d":"1.22"},{"v":1.215075930380339,"d":"1.22"},{"v":0.582284036,"d":"0.58"}]
["01061","Geneva","AL",{"v":0.228973261,"d":"0.23"},{"v":1.205733522951975,"d":"1.21"},{"v":1.205733522951975,"d":"1.21"},{"v":0.5262367115,"d":"0.53"}]
["01063","Greene","AL",{"v":0.21587767000000002,"d":"0.22"},{"v":1.2661599641445755,"d":"1.27"},{"v":1.2661599641445753,"d":"1.27"},{"v":0.6025559409999999,"d":"0.60"}]
["01065","Hale","AL",{"v":0.217602367,"d":"0.22"},{"v":1.2279714749396375,"d":"1.23"},{"v":1.2279714749396375,"d":"1.23"},{"v":0.5789798235,"d":"0.58"}]
["01067","Henry","AL",{"v":0.22640481599999998,"d":"0.23"},{"v":1.1939982587771207,"d":"1.19"},{"v":1.1939982587771207,"d":"1.19"},{"v":0.548616243,"d":"0.55"}]
["01069","Houston","AL",{"v":0.192954517,"d":"0.19"},{"v":1.169795232096763,"d":"1.17"},{"v":1.169795232096763,"d":"1.17"},{"v":0.4569932104999999,"d":"0.46"}]
["01071","Jackson","AL",{"v":0.20748176000000002,"d":"0.21"},{"v":1.258312059592945,"d":"1.26"},{"v":1.2583120595929451,"d":"1.26"},{"v":0.5776222145,"d":"0.58"}]
["01073","Jefferson","AL",{"v":0.141516703,"d":"0.14"},{"v":1.083997154382826,"d":"1.08"},{"v":1.083997154382826,"d":"1.08"},{"v":0.5039947745,"d":"0.50"}]
["01075","Lamar","AL",{"v":0.214659761,"d":"0.21"},{"v":1.1795107340481512,"d":"1.18"},{"v":1.179510734048151,"d":"1.18"},{"v":0.6537401465,"d":"0.65"}]
["01077","Lauderdale","AL",{"v":0.19530214,"d":"0.20"},{"v":1.2160817829557171,"d":"1.22"},{"v":1.2160817829557171,"d":"1.22"},{"v":0.4891290615000001,"d":"0.49"}]
["01079","Lawrence","AL",{"v":0.22292386599999997,"d":"0.22"},{"v":1.2716759899469352,"d":"1.27"},{"v":1.2716759899469354,"d":"1.27"},{"v":0.543233476,"d":"0.54"}]
["01081","Lee","AL",{"v":0.164415159,"d":"0.16"},{"v":1.1817863713513623,"d":"1.18"},{"v":1.1817863713513623,"d":"1.18"},{"v":0.5330304735000001,"d":"0.53"}]
["01083","Limestone","AL",{"v":0.206599024,"d":"0.21"},{"v":1.2487789990449705,"d":"1.25"},{"v":1.2487789990449703,"d":"1.25"},{"v":0.47044689649999993,"d":"0.47"}]
["01085","Lowndes","AL",{"v":0.22755524299999996,"d":"0.23"},{"v":1.2410434165162347,"d":"1.24"},{"v":1.2410434165162347,"d":"1.24"},{"v":0.5885624835,"d":"0.59"}]
["01087","Macon","AL",{"v":0.20099655400000002,"d":"0.20"},{"v":1.1608320607954485,"d":"1.16"},{"v":1.1608320607954483,"d":"1.16"},{"v":0.5774672289999999,"d":"0.58"}]
["01089","Madison","AL",{"v":0.16232440499999998,"d":"0.16"},{"v":1.183631500008354,"d":"1.18"},{"v":1.183631500008354,"d":"1.18"},{"v":0.441244441,"d":"0.44"}]
["01091","Marengo","AL",{"v":0.203921643,"d":"0.20"},{"v":1.207296726119023,"d":"1.21"},{"v":1.2072967261190228,"d":"1.21"},{"v":0.5938384474999999,"d":"0.59"}]
["01093","Marion","AL",{"v":0.21343258600000004,"d":"0.21"},{"v":1.1656320982412405,"d":"1.17"},{"v":1.1656320982412403,"d":"1.17"},{"v":0.6168689595,"d":"0.62"}]
["01095","Marshall","AL",{"v":0.19854622999999996,"d":"0.20"},{"v":1.2123752869079791,"d":"1.21"},{"v":1.2123752869079794,"d":"1.21"},{"v":0.5000307490000001,"d":"0.50"}]
["01097","Mobile","AL",{"v":0.173042543,"d":"0.17"},{"v":1.0633635957279117,"d":"1.06"},{"v":1.0633635957279117,"d":"1.06"},{"v":0.4515988735,"d":"0.45"}]
["01099","Monroe","AL",{"v":0.209634688,"d":"0.21"},{"v":1.2000743116958206,"d":"1.20"},{"v":1.2000743116958208,"d":"1.20"},{"v":0.606593039,"d":"0.61"}]
["01101","Montgomery","AL",{"v":0.16783453500000003,"d":"0.17"},{"v":1.0936945302213883,"d":"1.09"},{"v":1.0936945302213885,"d":"1.09"},{"v":0.46702949899999996,"d":"0.47"}]
["01103","Morgan","AL",{"v":0.186032643,"d":"0.19"},{"v":1.236468340815408,"d":"1.24"},{"v":1.2364683408154082,"d":"1.24"},{"v":0.4874579920000001,"d":"0.49"}]
["01105","Perry","AL",{"v":0.22450486,"d":"0.22"},{"v":1.2021604934143688,"d":"1.20"},{"v":1.2021604934143686,"d":"1.20"},{"v":0.6079710724999999,"d":"0.61"}]
["01107","Pickens","AL",{"v":0.21636172499999998,"d":"0.22"},{"v":1.2069460622327541,"d":"1.21"},{"v":1.2069460622327541,"d":"1.21"},{"v":0.6423738895000001,"d":"0.64"}]
["01109","Pike","AL",{"v":0.19558192999999996,"d":"0.20"},{"v":1.1743191456301636,"d":"1.17"},{"v":1.1743191456301636,"d":"1.17"},{"v":0.5629594485000001,"d":"0.56"}]
["01111","Randolph","AL",{"v":0.209779481,"d":"0.21"},{"v":1.2503021382236863,"d":"1.25"},{"v":1.2503021382236863,"d":"1.25"},{"v":0.59587815,"d":"0.60"}]
["01113","Russell","AL",{"v":0.185484277,"d":"0.19"},{"v":1.1562730126497758,"d":"1.16"},{"v":1.156273012649776,"d":"1.16"},{"v":0.5455747075,"d":"0.55"}]
["01115","St Clair","AL",{"v":0.198775722,"d":"0.20"},{"v":1.2317141009303563,"d":"1.23"},{"v":1.231714100930356,"d":"1.23"},{"v":0.5760644935,"d":"0.58"}]
["01117","Shelby","AL",{"v":0.17104013100000004,"d":"0.17"},{"v":1.1728720169524236,"d":"1.17"},{"v":1.1728720169524234,"d":"1.17"},{"v":0.5277955765000001,"d":"0.53"}]
["01119","Sumter","AL",{"v":0.2183211,"d":"0.22"},{"v":1.2349212958494542,"d":"1.23"},{"v":1.2349212958494542,"d":"1.23"},{"v":0.609218649,"d":"0.61"}]
["01121","Talladega","AL",{"v":0.194047155,"d":"0.19"},{"v":1.2209290382728775,"d":"1.22"},{"v":1.2209290382728777,"d":"1.22"},{"v":0.561186724,"d":"0.56"}]
["01123","Tallapoosa","AL",{"v":0.203887188,"d":"0.20"},{"v":1.2226067395844684,"d":"1.22"},{"v":1.2226067395844682,"d":"1.22"},{"v":0.6011960945,"d":"0.60"}]
["01125","Tuscaloosa","AL",{"v":0.16524557799999998,"d":"0.17"},{"v":1.1798236820596562,"d":"1.18"},{"v":1.1798236820596562,"d":"1.18"},{"v":0.560563698,"d":"0.56"}]
["01127","Walker","AL",{"v":0.201770192,"d":"0.20"},{"v":1.2597913122287694,"d":"1.26"},{"v":1.2597913122287694,"d":"1.26"},{"v":0.597815598,"d":"0.60"}]
["01129","Washington","AL",{"v":0.220269101,"d":"0.22"},{"v":1.216651137049633,"d":"1.22"},{"v":1.216651137049633,"d":"1.22"},{"v":0.6442220365,"d":"0.64"}]
["01131","Wilcox","AL",{"v":0.222408943,"d":"0.22"},{"v":1.2437245411685482,"d":"1.24"},{"v":1.2437245411685485,"d":"1.24"},{"v":0.6188585030000001,"d":"0.62"}]
["01133","Winston","AL",{"v":0.20963358499999998,"d":"0.21"},{"v":1.2460396254884305,"d":"1.25"},{"v":1.2460396254884305,"d":"1.25"},{"v":0.613919224,"d":"0.61"}]
["02013","Aleutians East","AK",{"v":0.016377968080965352,"d":"0.02"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.4094492020241339,"d":"0.41"}]
["02016","Aleutians West","AK",{"v":1.3102374464772284,"d":"1.31"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.0472460101206695,"d":"2.05"}]
["02020","Anchorage","AK",{"v":1.2283476060724015,"d":"1.23"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":4.913390424289606,"d":"4.91"}]
["02050","Bethel","AK",{"v":1.6377968080965355,"d":"1.64"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":4.094492020241339,"d":"4.09"}]
["02060","Bristol Bay","AK",{"v":1.6377968080965355,"d":"1.64"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":4.094492020241339,"d":"4.09"}]
["02068","Denali","AK",{"v":4.913390424289607,"d":"4.91"},{"v":6.551187232386142,"d":"6.55"},{"v":6.551187232386141,"d":"6.55"},{"v":5.32283962631374,"d":"5.32"}]
["02070","Dillingham","AK",{"v":1.6377968080965355,"d":"1.64"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":4.094492020241339,"d":"4.09"}]
["02090","Fairbanks North Star","AK",{"v":4.479240596167495,"d":"4.48"},{"v":5.972320794889993,"d":"5.97"},{"v":5.972320794889993,"d":"5.97"},{"v":4.8525106458481195,"d":"4.85"}]
["02100","Haines","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":3.275593616193071,"d":"3.28"},{"v":3.2755936161930705,"d":"3.28"},{"$error":"#DIV/0!"}]
["02105","Hoonah Angoon","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":3.2755936161930705,"d":"3.28"},{"v":3.2755936161930705,"d":"3.28"},{"v":2.4566952121448034,"d":"2.46"}]
["02110","Juneau","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":3.275593616193071,"d":"3.28"},{"v":3.2755936161930705,"d":"3.28"},{"v":2.4566952121448034,"d":"2.46"}]
["02122","Kenai Peninsula","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":4.913390424289606,"d":"4.91"},{"v":4.913390424289606,"d":"4.91"},{"v":3.234648695990657,"d":"3.23"}]
["02130","Ketchikan Gateway","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":3.275593616193071,"d":"3.28"},{"v":3.2755936161930714,"d":"3.28"},{"v":3.685042818217204,"d":"3.69"}]
["02150","Kodiak Island","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":4.913390424289607,"d":"4.91"},{"v":4.913390424289608,"d":"4.91"},{"v":3.234648695990657,"d":"3.23"}]
["02158","Kusilvak","AK",{"v":1.6377968080965355,"d":"1.64"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":4.094492020241339,"d":"4.09"}]
["02164","Lake and Peninsula","AK",{"v":1.6377968080965355,"d":"1.64"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":4.094492020241339,"d":"4.09"}]
["02170","Matanuska Susitna","AK",{"v":1.2283476060724017,"d":"1.23"},{"v":4.913390424289607,"d":"4.91"},{"v":4.913390424289606,"d":"4.91"},{"v":4.913390424289607,"d":"4.91"}]
["02180","Nome","AK",{"v":0.8188984040482677,"d":"0.82"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":4.094492020241339,"d":"4.09"}]
["02185","North Slope","AK",{"v":0,"d":"0.00"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02188","Northwest Arctic","AK",{"v":0.8188984040482676,"d":"0.82"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02195","Petersburg","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":3.2755936161930714,"d":"3.28"},{"v":3.275593616193071,"d":"3.28"},{"v":2.456695212144803,"d":"2.46"}]
["02198","Prince of Wales-Hyder","AK",{"v":0.8129649309245485,"d":"0.81"},{"v":3.251859723698194,"d":"3.25"},{"v":3.251859723698194,"d":"3.25"},{"v":2.4388947927736457,"d":"2.44"}]
["02220","Sitka","AK",{"v":0.8188984040482679,"d":"0.82"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.456695212144803,"d":"2.46"}]
["02230","Skagway","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":3.275593616193071,"d":"3.28"},{"v":3.2755936161930714,"d":"3.28"},{"v":2.456695212144803,"d":"2.46"}]
["02240","Southeast Fairbanks","AK",{"v":4.913390424289607,"d":"4.91"},{"v":6.551187232386142,"d":"6.55"},{"v":6.551187232386143,"d":"6.55"},{"v":5.32283962631374,"d":"5.32"}]
["02261","Valdez Cordova","AK",{"v":0.8188984040482677,"d":"0.82"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.4566952121448034,"d":"2.46"}]
["02275","Wrangell","AK",{"v":0.8129649309245485,"d":"0.81"},{"v":3.2518597236981943,"d":"3.25"},{"v":3.2518597236981934,"d":"3.25"},{"v":2.4388947927736453,"d":"2.44"}]
["02282","Yakutat","AK",{"v":0.8188984040482677,"d":"0.82"},{"v":3.2755936161930714,"d":"3.28"},{"v":3.2755936161930714,"d":"3.28"},{"v":2.4566952121448034,"d":"2.46"}]
["02290","Yukon Koyukuk","AK",{"v":1.6377968080965355,"d":"1.64"},{"v":6.551187232386142,"d":"6.55"},{"v":6.551187232386141,"d":"6.55"},{"v":4.094492020241339,"d":"4.09"}]
["04001","Apache","AZ",{"v":0.19453324399999997,"d":"0.19"},{"v":1.1565099890796657,"d":"1.16"},{"v":1.1565099890796657,"d":"1.16"},{"v":0.39712598400000004,"d":"0.40"}]
["04003","Cochise","AZ",{"v":0.189551935,"d":"0.19"},{"v":0.9528024872483997,"d":"0.95"},{"v":0.9528024872483998,"d":"0.95"},{"v":0.3247267575000001,"d":"0.32"}]
["04005","Coconino","AZ",{"v":0.174068245,"d":"0.17"},{"v":1.0958531816286958,"d":"1.10"},{"v":1.0958531816286958,"d":"1.10"},{"v":0.35842638699999996,"d":"0.36"}]
["04007","Gila","AZ",{"v":0.186374143,"d":"0.19"},{"v":1.0107440878754819,"d":"1.01"},{"v":1.0107440878754819,"d":"1.01"},{"v":0.35616068249999994,"d":"0.36"}]
["04009","Graham","AZ",{"v":0.19010639799999998,"d":"0.19"},{"v":0.9556303024015079,"d":"0.96"},{"v":0.9556303024015079,"d":"0.96"},{"v":0.33466570449999994,"d":"0.33"}]
["04011","Greenlee","AZ",{"v":0.18922016800000002,"d":"0.19"},{"v":0.9253601877146761,"d":"0.93"},{"v":0.9253601877146762,"d":"0.93"},{"v":0.3603278104999999,"d":"0.36"}]
["04012","La Paz","AZ",{"v":0.205109387,"d":"0.21"},{"v":1.013267672169219,"d":"1.01"},{"v":1.013267672169219,"d":"1.01"},{"v":0.32882558,"d":"0.33"}]
["04013","Maricopa","AZ",{"v":0.155104951,"d":"0.16"},{"v":0.902586693088236,"d":"0.90"},{"v":0.902586693088236,"d":"0.90"},{"v":0.267076935,"d":"0.27"}]
["04015","Mohave","AZ",{"v":0.18147945999999998,"d":"0.18"},{"v":1.0022229858917748,"d":"1.00"},{"v":1.0022229858917748,"d":"1.00"},{"v":0.31678250050000006,"d":"0.32"}]
["04017","Navajo","AZ",{"v":0.18577240800000003,"d":"0.19"},{"v":1.1284454863216662,"d":"1.13"},{"v":1.1284454863216662,"d":"1.13"},{"v":0.37358761850000005,"d":"0.37"}]
["04019","Pima","AZ",{"v":0.172741185,"d":"0.17"},{"v":0.9367246585927208,"d":"0.94"},{"v":0.9367246585927207,"d":"0.94"},{"v":0.289701327,"d":"0.29"}]
["04021","Pinal","AZ",{"v":0.18492084100000003,"d":"0.18"},{"v":0.9279437835704816,"d":"0.93"},{"v":0.9279437835704817,"d":"0.93"},{"v":0.29696336249999994,"d":"0.30"}]
["04023","Santa Cruz","AZ",{"v":0.19083293899999998,"d":"0.19"},{"v":0.9545665216763531,"d":"0.95"},{"v":0.954566521676353,"d":"0.95"},{"v":0.32328272500000005,"d":"0.32"}]
["04025","Yavapai","AZ",{"v":0.185680411,"d":"0.19"},{"v":0.9843185400480807,"d":"0.98"},{"v":0.9843185400480805,"d":"0.98"},{"v":0.3324552495,"d":"0.33"}]
["04027","Yuma","AZ",{"v":0.181272532,"d":"0.18"},{"v":0.9596171310081101,"d":"0.96"},{"v":0.9596171310081101,"d":"0.96"},{"v":0.285120404,"d":"0.29"}]
["05001","Arkansas","AR",{"v":0.45819972999999997,"d":"0.46"},{"v":2.730070869995396,"d":"2.73"},{"v":2.730070869995396,"d":"2.73"},{"v":1.063369224,"d":"1.06"}]
["05003","Ashley","AR",{"v":0.448562432,"d":"0.45"},{"v":2.713109569740535,"d":"2.71"},{"v":2.713109569740535,"d":"2.71"},{"v":1.2538010034999998,"d":"1.25"}]
["05005","Baxter","AR",{"v":0.451362472,"d":"0.45"},{"v":2.940236589979806,"d":"2.94"},{"v":2.940236589979806,"d":"2.94"},{"v":1.3078275155,"d":"1.31"}]
["05007","Benton","AR",{"v":0.40226906399999995,"d":"0.40"},{"v":2.811181575573064,"d":"2.81"},{"v":2.8111815755730643,"d":"2.81"},{"v":1.075162158,"d":"1.08"}]
["05009","Boone","AR",{"v":0.463786759,"d":"0.46"},{"v":2.933302553239544,"d":"2.93"},{"v":2.933302553239544,"d":"2.93"},{"v":1.193106732,"d":"1.19"}]
["05011","Bradley","AR",{"v":0.440928925,"d":"0.44"},{"v":2.750371480297453,"d":"2.75"},{"v":2.750371480297453,"d":"2.75"},{"v":1.3889892405000002,"d":"1.39"}]
["05013","Calhoun","AR",{"v":0.4944400329999999,"d":"0.49"},{"v":2.777650653418731,"d":"2.78"},{"v":2.777650653418731,"d":"2.78"},{"v":1.5039666834999998,"d":"1.50"}]
["05015","Carroll","AR",{"v":0.481577067,"d":"0.48"},{"v":2.976174695568773,"d":"2.98"},{"v":2.976174695568773,"d":"2.98"},{"v":1.2701103360000001,"d":"1.27"}]
["05017","Chicot","AR",{"v":0.5086418640000001,"d":"0.51"},{"v":2.695225139742209,"d":"2.70"},{"v":2.6952251397422087,"d":"2.70"},{"v":1.0154273809999999,"d":"1.02"}]
["05019","Clark","AR",{"v":0.4391032100000001,"d":"0.44"},{"v":2.6845891615572604,"d":"2.68"},{"v":2.68458916155726,"d":"2.68"},{"v":1.3913576525,"d":"1.39"}]
["05021","Clay","AR",{"v":0.498060303,"d":"0.50"},{"v":2.730315022562281,"d":"2.73"},{"v":2.730315022562281,"d":"2.73"},{"v":1.0510729535,"d":"1.05"}]
["05023","Cleburne","AR",{"v":0.466464605,"d":"0.47"},{"v":3.0198116006234335,"d":"3.02"},{"v":3.0198116006234335,"d":"3.02"},{"v":1.3339975130000001,"d":"1.33"}]
["05025","Cleveland","AR",{"v":0.486547363,"d":"0.49"},{"v":2.887382972573534,"d":"2.89"},{"v":2.8873829725735343,"d":"2.89"},{"v":1.521561178,"d":"1.52"}]
["05027","Columbia","AR",{"v":0.43237192599999996,"d":"0.43"},{"v":2.6980271536084115,"d":"2.70"},{"v":2.698027153608412,"d":"2.70"},{"v":1.4417829175,"d":"1.44"}]
["05029","Conway","AR",{"v":0.47350516500000006,"d":"0.47"},{"v":2.7948857116074537,"d":"2.79"},{"v":2.7948857116074537,"d":"2.79"},{"v":1.256403823,"d":"1.26"}]
["05031","Craighead","AR",{"v":0.449467894,"d":"0.45"},{"v":2.7266462863928798,"d":"2.73"},{"v":2.7266462863928798,"d":"2.73"},{"v":0.9563480544999999,"d":"0.96"}]
["05033","Crawford","AR",{"v":0.435459176,"d":"0.44"},{"v":2.7777540056470773,"d":"2.78"},{"v":2.777754005647078,"d":"2.78"},{"v":1.2793938155,"d":"1.28"}]
["05035","Crittenden","AR",{"v":0.45295088600000005,"d":"0.45"},{"v":2.630536613220867,"d":"2.63"},{"v":2.630536613220867,"d":"2.63"},{"v":0.9091906974999998,"d":"0.91"}]
["05037","Cross","AR",{"v":0.505141249,"d":"0.51"},{"v":2.76045852818473,"d":"2.76"},{"v":2.76045852818473,"d":"2.76"},{"v":1.022352809,"d":"1.02"}]
["05039","Dallas","AR",{"v":0.437878609,"d":"0.44"},{"v":2.7410349402007927,"d":"2.74"},{"v":2.7410349402007927,"d":"2.74"},{"v":1.4326609485,"d":"1.43"}]
["05041","Desha","AR",{"v":0.46519925100000004,"d":"0.47"},{"v":2.6348365756072645,"d":"2.63"},{"v":2.6348365756072645,"d":"2.63"},{"v":1.0239360975,"d":"1.02"}]
["05043","Drew","AR",{"v":0.43359198000000004,"d":"0.43"},{"v":2.8018920378220344,"d":"2.80"},{"v":2.8018920378220344,"d":"2.80"},{"v":1.273723741,"d":"1.27"}]
["05045","Faulkner","AR",{"v":0.4127487899999999,"d":"0.41"},{"v":2.705038220906517,"d":"2.71"},{"v":2.705038220906517,"d":"2.71"},{"v":1.1162087445,"d":"1.12"}]
["05047","Franklin","AR",{"v":0.491250964,"d":"0.49"},{"v":2.835740455017253,"d":"2.84"},{"v":2.8357404550172527,"d":"2.84"},{"v":1.286066127,"d":"1.29"}]
["05049","Fulton","AR",{"v":0.505490733,"d":"0.51"},{"v":3.082503550996142,"d":"3.08"},{"v":3.082503550996141,"d":"3.08"},{"v":1.2819964700000004,"d":"1.28"}]
["05051","Garland","AR",{"v":0.399373043,"d":"0.40"},{"v":2.791375155487764,"d":"2.79"},{"v":2.7913751554877635,"d":"2.79"},{"v":1.314805187,"d":"1.31"}]
["05053","Grant","AR",{"v":0.452908526,"d":"0.45"},{"v":2.798850713290361,"d":"2.80"},{"v":2.798850713290361,"d":"2.80"},{"v":1.4358371849999998,"d":"1.44"}]
["05055","Greene","AR",{"v":0.466470869,"d":"0.47"},{"v":2.8680418401759655,"d":"2.87"},{"v":2.868041840175966,"d":"2.87"},{"v":1.0319032264999999,"d":"1.03"}]
["05057","Hempstead","AR",{"v":0.46396918700000006,"d":"0.46"},{"v":2.6655271413003,"d":"2.67"},{"v":2.6655271413003003,"d":"2.67"},{"v":1.2511206605,"d":"1.25"}]
["05059","Hot Spring","AR",{"v":0.450161742,"d":"0.45"},{"v":2.84528538860085,"d":"2.85"},{"v":2.84528538860085,"d":"2.85"},{"v":1.3894162315,"d":"1.39"}]
["05061","Howard","AR",{"v":0.473047738,"d":"0.47"},{"v":2.6815950320731177,"d":"2.68"},{"v":2.681595032073118,"d":"2.68"},{"v":1.3047795135,"d":"1.30"}]
["05063","Independence","AR",{"v":0.47111894300000007,"d":"0.47"},{"v":2.8717216971817137,"d":"2.87"},{"v":2.8717216971817137,"d":"2.87"},{"v":1.2346901700000001,"d":"1.23"}]
["05065","Izard","AR",{"v":0.501790231,"d":"0.50"},{"v":3.0648302113083026,"d":"3.06"},{"v":3.0648302113083026,"d":"3.06"},{"v":1.375308339,"d":"1.38"}]
["05067","Jackson","AR",{"v":0.503878169,"d":"0.50"},{"v":2.6860725390570375,"d":"2.69"},{"v":2.6860725390570366,"d":"2.69"},{"v":1.0383029329999998,"d":"1.04"}]
["05069","Jefferson","AR",{"v":0.439500756,"d":"0.44"},{"v":2.616703944138341,"d":"2.62"},{"v":2.616703944138341,"d":"2.62"},{"v":1.057742419,"d":"1.06"}]
["05071","Johnson","AR",{"v":0.455387515,"d":"0.46"},{"v":2.8553185117017663,"d":"2.86"},{"v":2.8553185117017663,"d":"2.86"},{"v":1.3975336329999999,"d":"1.40"}]
["05073","Lafayette","AR",{"v":0.519180275,"d":"0.52"},{"v":2.7651454756790943,"d":"2.77"},{"v":2.765145475679094,"d":"2.77"},{"v":1.3411001415,"d":"1.34"}]
["05075","Lawrence","AR",{"v":0.495080149,"d":"0.50"},{"v":2.762294370017272,"d":"2.76"},{"v":2.762294370017272,"d":"2.76"},{"v":1.0968005445,"d":"1.10"}]
["05077","Lee","AR",{"v":0.496999007,"d":"0.50"},{"v":2.65720191260313,"d":"2.66"},{"v":2.65720191260313,"d":"2.66"},{"v":1.0424528769999999,"d":"1.04"}]
["05079","Lincoln","AR",{"v":0.530212737,"d":"0.53"},{"v":2.826965468274287,"d":"2.83"},{"v":2.826965468274287,"d":"2.83"},{"v":1.201991365,"d":"1.20"}]
["05081","Little River","AR",{"v":0.4795104799999999,"d":"0.48"},{"v":2.7398896919953377,"d":"2.74"},{"v":2.7398896919953373,"d":"2.74"},{"v":1.2507096880000004,"d":"1.25"}]
["05083","Logan","AR",{"v":0.474690204,"d":"0.47"},{"v":2.823580525244496,"d":"2.82"},{"v":2.823580525244496,"d":"2.82"},{"v":1.2971975435,"d":"1.30"}]
["05085","Lonoke","AR",{"v":0.47604802500000004,"d":"0.48"},{"v":2.7468620461885656,"d":"2.75"},{"v":2.746862046188566,"d":"2.75"},{"v":1.014188788,"d":"1.01"}]
["05087","Madison","AR",{"v":0.4943337890000001,"d":"0.49"},{"v":3.068264444523604,"d":"3.07"},{"v":3.0682644445236034,"d":"3.07"},{"v":1.4146978675,"d":"1.41"}]
["05089","Marion","AR",{"v":0.510066564,"d":"0.51"},{"v":3.0588200335445856,"d":"3.06"},{"v":3.0588200335445856,"d":"3.06"},{"v":1.3378082994999998,"d":"1.34"}]
["05091","Miller","AR",{"v":0.434136936,"d":"0.43"},{"v":2.6586851944903556,"d":"2.66"},{"v":2.658685194490356,"d":"2.66"},{"v":1.1252130955,"d":"1.13"}]
["05093","Mississippi","AR",{"v":0.48169885400000007,"d":"0.48"},{"v":2.5888217514417846,"d":"2.59"},{"v":2.5888217514417846,"d":"2.59"},{"v":0.9538578415,"d":"0.95"}]
["05095","Monroe","AR",{"v":0.499248595,"d":"0.50"},{"v":2.6248774675098567,"d":"2.62"},{"v":2.624877467509857,"d":"2.62"},{"v":1.154703166,"d":"1.15"}]
["05097","Montgomery","AR",{"v":0.49200415,"d":"0.49"},{"v":2.9273708787834534,"d":"2.93"},{"v":2.9273708787834534,"d":"2.93"},{"v":1.50026117,"d":"1.50"}]
["05099","Nevada","AR",{"v":0.462035494,"d":"0.46"},{"v":2.753819492306773,"d":"2.75"},{"v":2.753819492306773,"d":"2.75"},{"v":1.4074048479999999,"d":"1.41"}]
["05101","Newton","AR",{"v":0.47354844800000007,"d":"0.47"},{"v":3.163481820339923,"d":"3.16"},{"v":3.1634818203399226,"d":"3.16"},{"v":1.5846165615,"d":"1.58"}]
["05103","Ouachita","AR",{"v":0.435998079,"d":"0.44"},{"v":2.6006974945286827,"d":"2.60"},{"v":2.600697494528683,"d":"2.60"},{"v":1.460242643,"d":"1.46"}]
["05105","Perry","AR",{"v":0.492025691,"d":"0.49"},{"v":2.9547583841902534,"d":"2.95"},{"v":2.954758384190254,"d":"2.95"},{"v":1.4553857340000003,"d":"1.46"}]
["05107","Phillips","AR",{"v":0.48060511400000006,"d":"0.48"},{"v":2.473498904706521,"d":"2.47"},{"v":2.4734989047065215,"d":"2.47"},{"v":1.0472129305,"d":"1.05"}]
["05109","Pike","AR",{"v":0.502068916,"d":"0.50"},{"v":2.775221278757516,"d":"2.78"},{"v":2.775221278757516,"d":"2.78"},{"v":1.4211899830000003,"d":"1.42"}]
["05111","Poinsett","AR",{"v":0.524748236,"d":"0.52"},{"v":2.6977089476859573,"d":"2.70"},{"v":2.6977089476859573,"d":"2.70"},{"v":1.0508278125000001,"d":"1.05"}]
["05113","Polk","AR",{"v":0.45550832900000005,"d":"0.46"},{"v":2.9475969490213725,"d":"2.95"},{"v":2.9475969490213725,"d":"2.95"},{"v":1.4203073410000002,"d":"1.42"}]
["05115","Pope","AR",{"v":0.43886805200000006,"d":"0.44"},{"v":2.836065554235573,"d":"2.84"},{"v":2.8360655542355726,"d":"2.84"},{"v":1.3350555485000004,"d":"1.34"}]
["05117","Prairie","AR",{"v":0.545146872,"d":"0.55"},{"v":2.8401534524936056,"d":"2.84"},{"v":2.840153452493606,"d":"2.84"},{"v":1.1603960335,"d":"1.16"}]
["05119","Pulaski","AR",{"v":0.341474224,"d":"0.34"},{"v":2.5105138074250655,"d":"2.51"},{"v":2.5105138074250655,"d":"2.51"},{"v":1.0430183445,"d":"1.04"}]
["05121","Randolph","AR",{"v":0.48167705,"d":"0.48"},{"v":2.804020252605312,"d":"2.80"},{"v":2.804020252605312,"d":"2.80"},{"v":1.2116926264999999,"d":"1.21"}]
["05123","St Francis","AR",{"v":0.502831997,"d":"0.50"},{"v":2.6953553427022676,"d":"2.70"},{"v":2.6953553427022676,"d":"2.70"},{"v":1.0505299205,"d":"1.05"}]
["05125","Saline","AR",{"v":0.3956542679999999,"d":"0.40"},{"v":2.7443481198362045,"d":"2.74"},{"v":2.7443481198362045,"d":"2.74"},{"v":1.318235844,"d":"1.32"}]
["05127","Scott","AR",{"v":0.4501580029999999,"d":"0.45"},{"v":2.915911533026806,"d":"2.92"},{"v":2.915911533026806,"d":"2.92"},{"v":1.4823181165,"d":"1.48"}]
["05129","Searcy","AR",{"v":0.4968233570000001,"d":"0.50"},{"v":3.1256387629959046,"d":"3.13"},{"v":3.125638762995905,"d":"3.13"},{"v":1.4136820465,"d":"1.41"}]
["05131","Sebastian","AR",{"v":0.400918188,"d":"0.40"},{"v":2.634825321330766,"d":"2.63"},{"v":2.6348253213307657,"d":"2.63"},{"v":1.0608682559999998,"d":"1.06"}]
["05133","Sevier","AR",{"v":0.4688302610000001,"d":"0.47"},{"v":2.8298207652666307,"d":"2.83"},{"v":2.829820765266631,"d":"2.83"},{"v":1.3069077825,"d":"1.31"}]
["05135","Sharp","AR",{"v":0.47345701999999995,"d":"0.47"},{"v":3.074849678762993,"d":"3.07"},{"v":3.074849678762993,"d":"3.07"},{"v":1.3804211720000001,"d":"1.38"}]
["05137","Stone","AR",{"v":0.481907462,"d":"0.48"},{"v":3.1375828090260067,"d":"3.14"},{"v":3.137582809026007,"d":"3.14"},{"v":1.473085323,"d":"1.47"}]
["05139","Union","AR",{"v":0.42914531000000006,"d":"0.43"},{"v":2.6639905082086033,"d":"2.66"},{"v":2.6639905082086033,"d":"2.66"},{"v":1.4312481705,"d":"1.43"}]
["05141","Van Buren","AR",{"v":0.475837106,"d":"0.48"},{"v":3.1151079502071797,"d":"3.12"},{"v":3.11510795020718,"d":"3.12"},{"v":1.4640189005,"d":"1.46"}]
["05143","Washington","AR",{"v":0.37992197800000005,"d":"0.38"},{"v":2.747064950823441,"d":"2.75"},{"v":2.747064950823441,"d":"2.75"},{"v":1.1475473005000003,"d":"1.15"}]
["05145","White","AR",{"v":0.452883215,"d":"0.45"},{"v":2.8730998185136123,"d":"2.87"},{"v":2.8730998185136123,"d":"2.87"},{"v":1.163678769,"d":"1.16"}]
["05147","Woodruff","AR",{"v":0.557587993,"d":"0.56"},{"v":2.676461654252375,"d":"2.68"},{"v":2.6764616542523756,"d":"2.68"},{"v":1.117110505,"d":"1.12"}]
["05149","Yell","AR",{"v":0.46756555099999997,"d":"0.47"},{"v":2.8943137927858698,"d":"2.89"},{"v":2.89431379278587,"d":"2.89"},{"v":1.434649015,"d":"1.43"}]
["06001","Alameda","CA",{"v":0.24145787899999996,"d":"0.24"},{"v":0.16497485460276648,"d":"0.16"},{"v":0.16497485460276648,"d":"0.16"},{"v":0.7333533615,"d":"0.73"}]
["06003","Alpine","CA",{"v":0.5282610309999999,"d":"0.53"},{"v":3.700465896387969,"d":"3.70"},{"v":3.700465896387969,"d":"3.70"},{"v":1.3388233075,"d":"1.34"}]
["06005","Amador","CA",{"v":0.542186515,"d":"0.54"},{"v":2.9960666563526064,"d":"3.00"},{"v":2.996066656352606,"d":"3.00"},{"v":1.2060588505,"d":"1.21"}]
["06007","Butte","CA",{"v":0.447014526,"d":"0.45"},{"v":3.019486767683813,"d":"3.02"},{"v":3.0194867676838126,"d":"3.02"},{"v":1.1384293475,"d":"1.14"}]
["06009","Calaveras","CA",{"v":0.555734015,"d":"0.56"},{"v":3.0485221301559515,"d":"3.05"},{"v":3.048522130155952,"d":"3.05"},{"v":1.2347237649999998,"d":"1.23"}]
["06011","Colusa","CA",{"v":0.5215386610000001,"d":"0.52"},{"v":3.006806256044859,"d":"3.01"},{"v":3.0068062560448596,"d":"3.01"},{"v":1.0491766850000002,"d":"1.05"}]
["06013","Contra Costa","CA",{"v":0.302079153,"d":"0.30"},{"v":1.0443193735578113,"d":"1.04"},{"v":1.0443193735578116,"d":"1.04"},{"v":0.7797802505,"d":"0.78"}]
["06015","Del Norte","CA",{"v":0.46560435899999997,"d":"0.47"},{"v":3.3520266108760035,"d":"3.35"},{"v":3.352026610876003,"d":"3.35"},{"v":1.367657915,"d":"1.37"}]
["06017","El Dorado","CA",{"v":0.466215101,"d":"0.47"},{"v":3.0964582126341584,"d":"3.10"},{"v":3.0964582126341584,"d":"3.10"},{"v":1.2314107705000004,"d":"1.23"}]
["06019","Fresno","CA",{"v":0.46120433600000005,"d":"0.46"},{"v":2.788543579373105,"d":"2.79"},{"v":2.788543579373105,"d":"2.79"},{"v":0.985632022,"d":"0.99"}]
["06021","Glenn","CA",{"v":0.51076407,"d":"0.51"},{"v":3.051697695981316,"d":"3.05"},{"v":3.051697695981316,"d":"3.05"},{"v":1.1246618135,"d":"1.12"}]
["06023","Humboldt","CA",{"v":0.45687149900000007,"d":"0.46"},{"v":3.0357735453468613,"d":"3.04"},{"v":3.0357735453468613,"d":"3.04"},{"v":1.3616378615,"d":"1.36"}]
["06025","Imperial","CA",{"v":0.525785617,"d":"0.53"},{"v":2.7814935066840953,"d":"2.78"},{"v":2.781493506684096,"d":"2.78"},{"v":0.866255293,"d":"0.87"}]
["06027","Inyo","CA",{"v":0.5818809279999999,"d":"0.58"},{"v":2.906648764851437,"d":"2.91"},{"v":2.906648764851437,"d":"2.91"},{"v":0.9561731890000001,"d":"0.96"}]
["06029","Kern","CA",{"v":0.48740031599999994,"d":"0.49"},{"v":2.745247514417444,"d":"2.75"},{"v":2.7452475144174446,"d":"2.75"},{"v":0.9272489650000001,"d":"0.93"}]
["06031","Kings","CA",{"v":0.494228629,"d":"0.49"},{"v":2.7089628414762394,"d":"2.71"},{"v":2.7089628414762394,"d":"2.71"},{"v":0.9261660995,"d":"0.93"}]
["06033","Lake","CA",{"v":0.47968901699999994,"d":"0.48"},{"v":3.260458504353723,"d":"3.26"},{"v":3.260458504353723,"d":"3.26"},{"v":1.1549234764999998,"d":"1.15"}]
["06035","Lassen","CA",{"v":0.511810825,"d":"0.51"},{"v":3.5781509659409174,"d":"3.58"},{"v":3.578150965940918,"d":"3.58"},{"v":1.1951634375000002,"d":"1.20"}]
["06037","Los Angeles","CA",{"v":0.215570561,"d":"0.22"},{"v":0.10929628725937737,"d":"0.11"},{"v":0.10929628725937739,"d":"0.11"},{"v":0.6694899474999998,"d":"0.67"}]
["06039","Madera","CA",{"v":0.504024435,"d":"0.50"},{"v":2.9518467840747764,"d":"2.95"},{"v":2.9518467840747764,"d":"2.95"},{"v":1.1147343429999998,"d":"1.11"}]
["06041","Marin","CA",{"v":0.40503838300000006,"d":"0.41"},{"v":2.822181004321674,"d":"2.82"},{"v":2.822181004321674,"d":"2.82"},{"v":0.9409123379999998,"d":"0.94"}]
["06043","Mariposa","CA",{"v":0.590345134,"d":"0.59"},{"v":3.1233639978177763,"d":"3.12"},{"v":3.1233639978177767,"d":"3.12"},{"v":1.2715394295,"d":"1.27"}]
["06045","Mendocino","CA",{"v":0.4823378709999999,"d":"0.48"},{"v":3.198727298849799,"d":"3.20"},{"v":3.1987272988498,"d":"3.20"},{"v":1.3329142509999998,"d":"1.33"}]
["06047","Merced","CA",{"v":0.483087024,"d":"0.48"},{"v":2.8274219846181947,"d":"2.83"},{"v":2.8274219846181947,"d":"2.83"},{"v":0.9488629849999999,"d":"0.95"}]
["06049","Modoc","CA",{"v":0.564438609,"d":"0.56"},{"v":3.2214117971624243,"d":"3.22"},{"v":3.2214117971624248,"d":"3.22"},{"v":1.1270254525,"d":"1.13"}]
["06051","Mono","CA",{"v":0.530611434,"d":"0.53"},{"v":3.6109234948097915,"d":"3.61"},{"v":3.6109234948097915,"d":"3.61"},{"v":1.1291673665000002,"d":"1.13"}]
["06053","Monterey","CA",{"v":0.486050328,"d":"0.49"},{"v":2.716550327596328,"d":"2.72"},{"v":2.7165503275963285,"d":"2.72"},{"v":0.932026462,"d":"0.93"}]
["06055","Napa","CA",{"v":0.449442084,"d":"0.45"},{"v":2.972791586834442,"d":"2.97"},{"v":2.972791586834442,"d":"2.97"},{"v":1.0469012675000002,"d":"1.05"}]
["06057","Nevada","CA",{"v":0.4732524659999999,"d":"0.47"},{"v":3.1106702598351124,"d":"3.11"},{"v":3.1106702598351124,"d":"3.11"},{"v":1.261716147,"d":"1.26"}]
["06059","Orange","CA",{"v":0.14442866,"d":"0.14"},{"v":0.000896745832158789,"d":"0.00"},{"v":8.9674583215878915E-4,"d":"0.00"},{"v":0.5825334679999999,"d":"0.58"}]
["06061","Placer","CA",{"v":0.423710084,"d":"0.42"},{"v":2.9265467972569725,"d":"2.93"},{"v":2.9265467972569725,"d":"2.93"},{"v":1.1179538285,"d":"1.12"}]
["06063","Plumas","CA",{"v":0.541337696,"d":"0.54"},{"v":3.278675583765657,"d":"3.28"},{"v":3.278675583765657,"d":"3.28"},{"v":1.307900108,"d":"1.31"}]
["06065","Riverside","CA",{"v":0.47166447800000005,"d":"0.47"},{"v":2.566537344827683,"d":"2.57"},{"v":2.566537344827683,"d":"2.57"},{"v":0.811554553,"d":"0.81"}]
["06067","Sacramento","CA",{"v":0.30196366100000005,"d":"0.30"},{"v":1.046813018248802,"d":"1.05"},{"v":1.046813018248802,"d":"1.05"},{"v":0.7527935110000001,"d":"0.75"}]
["06069","San Benito","CA",{"v":0.539189219,"d":"0.54"},{"v":2.687947785345685,"d":"2.69"},{"v":2.6879477853456843,"d":"2.69"},{"v":0.9635003864999999,"d":"0.96"}]
["06071","San Bernardino","CA",{"v":0.505042428,"d":"0.51"},{"v":2.565273003236194,"d":"2.57"},{"v":2.565273003236194,"d":"2.57"},{"v":0.8307275369999999,"d":"0.83"}]
["06073","San Diego","CA",{"v":0.39366268200000004,"d":"0.39"},{"v":2.4536199163310584,"d":"2.45"},{"v":2.4536199163310584,"d":"2.45"},{"v":0.7781921895,"d":"0.78"}]
["06075","San Francisco","CA",{"v":1.339776E-3,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.30270824150000003,"d":"0.30"}]
["06077","San Joaquin","CA",{"v":0.41825515300000005,"d":"0.42"},{"v":2.6994063057837487,"d":"2.70"},{"v":2.699406305783749,"d":"2.70"},{"v":0.9158347879999998,"d":"0.92"}]
["06079","San Luis Obispo","CA",{"v":0.5113309849999998,"d":"0.51"},{"v":2.6550372468835115,"d":"2.66"},{"v":2.655037246883511,"d":"2.66"},{"v":0.9252718615000001,"d":"0.93"}]
["06081","San Mateo","CA",{"v":0.27343999099999994,"d":"0.27"},{"v":0.8045686440203798,"d":"0.80"},{"v":0.8045686440203796,"d":"0.80"},{"v":0.828951425,"d":"0.83"}]
["06083","Santa Barbara","CA",{"v":0.48176530200000006,"d":"0.48"},{"v":2.5456247263396414,"d":"2.55"},{"v":2.545624726339641,"d":"2.55"},{"v":0.8785497444999999,"d":"0.88"}]
["06085","Santa Clara","CA",{"v":0.299336097,"d":"0.30"},{"v":1.4398898927761805,"d":"1.44"},{"v":1.4398898927761805,"d":"1.44"},{"v":0.8327077165,"d":"0.83"}]
["06087","Santa Cruz","CA",{"v":0.40256696200000003,"d":"0.40"},{"v":2.575574228606436,"d":"2.58"},{"v":2.5755742286064356,"d":"2.58"},{"v":1.034583647,"d":"1.03"}]
["06089","Shasta","CA",{"v":0.466066172,"d":"0.47"},{"v":3.0622803443121844,"d":"3.06"},{"v":3.0622803443121853,"d":"3.06"},{"v":1.223344573,"d":"1.22"}]
["06091","Sierra","CA",{"v":0.578117445,"d":"0.58"},{"v":3.274198327797173,"d":"3.27"},{"v":3.274198327797173,"d":"3.27"},{"v":1.3297608185000003,"d":"1.33"}]
["06093","Siskiyou","CA",{"v":0.510689572,"d":"0.51"},{"v":3.3305989928728645,"d":"3.33"},{"v":3.3305989928728645,"d":"3.33"},{"v":1.3324644605,"d":"1.33"}]
["06095","Solano","CA",{"v":0.412071925,"d":"0.41"},{"v":2.795942214317329,"d":"2.80"},{"v":2.795942214317329,"d":"2.80"},{"v":0.867569026,"d":"0.87"}]
["06097","Sonoma","CA",{"v":0.42942923000000005,"d":"0.43"},{"v":2.9582737651606963,"d":"2.96"},{"v":2.958273765160696,"d":"2.96"},{"v":1.0609144835,"d":"1.06"}]
["06099","Stanislaus","CA",{"v":0.434081275,"d":"0.43"},{"v":2.6952625578285403,"d":"2.70"},{"v":2.69526255782854,"d":"2.70"},{"v":0.956603403,"d":"0.96"}]
["06101","Sutter","CA",{"v":0.472491946,"d":"0.47"},{"v":2.913497437357079,"d":"2.91"},{"v":2.9134974373570794,"d":"2.91"},{"v":0.9686883205,"d":"0.97"}]
["06103","Tehama","CA",{"v":0.515524955,"d":"0.52"},{"v":3.163745152794154,"d":"3.16"},{"v":3.163745152794154,"d":"3.16"},{"v":1.1666376655,"d":"1.17"}]
["06105","Trinity","CA",{"v":0.535804467,"d":"0.54"},{"v":3.4213972909766244,"d":"3.42"},{"v":3.421397290976624,"d":"3.42"},{"v":1.51832864,"d":"1.52"}]
["06107","Tulare","CA",{"v":0.477773995,"d":"0.48"},{"v":2.7423875182039077,"d":"2.74"},{"v":2.742387518203908,"d":"2.74"},{"v":1.0457630335,"d":"1.05"}]
["06109","Tuolumne","CA",{"v":0.512839802,"d":"0.51"},{"v":3.0962212608100623,"d":"3.10"},{"v":3.0962212608100623,"d":"3.10"},{"v":1.1770111890000001,"d":"1.18"}]
["06111","Ventura","CA",{"v":0.45058493000000005,"d":"0.45"},{"v":2.544805466380896,"d":"2.54"},{"v":2.544805466380896,"d":"2.54"},{"v":0.8365287605000001,"d":"0.84"}]
["06113","Yolo","CA",{"v":0.454489833,"d":"0.45"},{"v":2.933387878909433,"d":"2.93"},{"v":2.933387878909433,"d":"2.93"},{"v":0.9159223074999999,"d":"0.92"}]
["06115","Yuba","CA",{"v":0.46540787800000005,"d":"0.47"},{"v":3.000562493589697,"d":"3.00"},{"v":3.0005624935896966,"d":"3.00"},{"v":1.1454626075,"d":"1.15"}]
["08001","Adams","CO",{"v":0.299428385,"d":"0.30"},{"v":2.489506678773552,"d":"2.49"},{"v":2.4895066787735516,"d":"2.49"},{"v":0.6849717095,"d":"0.68"}]
["08003","Alamosa","CO",{"v":0.349390353,"d":"0.35"},{"v":2.7428748839224215,"d":"2.74"},{"v":2.742874883922421,"d":"2.74"},{"v":0.863666122,"d":"0.86"}]
["08005","Arapahoe","CO",{"v":0.261448395,"d":"0.26"},{"v":2.253996699769574,"d":"2.25"},{"v":2.253996699769574,"d":"2.25"},{"v":0.6532494845,"d":"0.65"}]
["08007","Archuleta","CO",{"v":0.357217841,"d":"0.36"},{"v":2.7867468174521424,"d":"2.79"},{"v":2.786746817452142,"d":"2.79"},{"v":1.0163894605000001,"d":"1.02"}]
["08009","Baca","CO",{"v":0.4620088050000001,"d":"0.46"},{"v":2.429375364926266,"d":"2.43"},{"v":2.429375364926266,"d":"2.43"},{"v":0.8675492939999998,"d":"0.87"}]
["08011","Bent","CO",{"v":0.398663893,"d":"0.40"},{"v":2.4379626264601484,"d":"2.44"},{"v":2.437962626460149,"d":"2.44"},{"v":0.7920647125000001,"d":"0.79"}]
["08013","Boulder","CO",{"v":0.283805185,"d":"0.28"},{"v":2.4941865608494087,"d":"2.49"},{"v":2.4941865608494087,"d":"2.49"},{"v":0.795159376,"d":"0.80"}]
["08014","Broomfield","CO",{"v":0.179014171,"d":"0.18"},{"v":0.1355795107812774,"d":"0.14"},{"v":0.1355795107812774,"d":"0.14"},{"v":0.5907517125,"d":"0.59"}]
["08015","Chaffee","CO",{"v":0.36919881099999996,"d":"0.37"},{"v":2.4781161321225293,"d":"2.48"},{"v":2.4781161321225293,"d":"2.48"},{"v":0.8820858775000001,"d":"0.88"}]
["08017","Cheyenne","CO",{"v":0.4573512699999999,"d":"0.46"},{"v":2.506344830135116,"d":"2.51"},{"v":2.5063448301351157,"d":"2.51"},{"v":0.8726299699999999,"d":"0.87"}]
["08019","Clear Creek","CO",{"v":0.409404761,"d":"0.41"},{"v":2.7035825260267203,"d":"2.70"},{"v":2.7035825260267203,"d":"2.70"},{"v":1.066228369,"d":"1.07"}]
["08021","Conejos","CO",{"v":0.410000898,"d":"0.41"},{"v":2.8561041502764595,"d":"2.86"},{"v":2.85610415027646,"d":"2.86"},{"v":1.0104634355,"d":"1.01"}]
["08023","Costilla","CO",{"v":0.408604502,"d":"0.41"},{"v":2.9219418801180788,"d":"2.92"},{"v":2.921941880118079,"d":"2.92"},{"v":1.013553241,"d":"1.01"}]
["08025","Crowley","CO",{"v":0.458157054,"d":"0.46"},{"v":2.465124709266173,"d":"2.47"},{"v":2.465124709266173,"d":"2.47"},{"v":0.8677037385,"d":"0.87"}]
["08027","Custer","CO",{"v":0.430629708,"d":"0.43"},{"v":2.638735527930373,"d":"2.64"},{"v":2.638735527930373,"d":"2.64"},{"v":0.9704234279999998,"d":"0.97"}]
["08029","Delta","CO",{"v":0.372246098,"d":"0.37"},{"v":2.7300614443563065,"d":"2.73"},{"v":2.7300614443563065,"d":"2.73"},{"v":0.9586387349999997,"d":"0.96"}]
["08031","Denver","CO",{"v":0.077357047,"d":"0.08"},{"v":2.4245138139451971E-6,"d":"0.00"},{"v":2.4245138139451971E-6,"d":"0.00"},{"v":0.47409082650000006,"d":"0.47"}]
["08033","Dolores","CO",{"v":0.407575347,"d":"0.41"},{"v":2.837831445664955,"d":"2.84"},{"v":2.837831445664955,"d":"2.84"},{"v":1.0460791515,"d":"1.05"}]
["08035","Douglas","CO",{"v":0.29864095300000004,"d":"0.30"},{"v":2.4983659224400387,"d":"2.50"},{"v":2.4983659224400387,"d":"2.50"},{"v":0.7815433255,"d":"0.78"}]
["08037","Eagle","CO",{"v":0.327703946,"d":"0.33"},{"v":2.8112459349434946,"d":"2.81"},{"v":2.8112459349434946,"d":"2.81"},{"v":0.897318329,"d":"0.90"}]
["08039","Elbert","CO",{"v":0.459441977,"d":"0.46"},{"v":2.5126259849281194,"d":"2.51"},{"v":2.5126259849281194,"d":"2.51"},{"v":0.8659513369999998,"d":"0.87"}]
["08041","El Paso","CO",{"v":0.325173622,"d":"0.33"},{"v":2.3602617398530232,"d":"2.36"},{"v":2.3602617398530237,"d":"2.36"},{"v":0.7045355259999999,"d":"0.70"}]
["08043","Fremont","CO",{"v":0.35917023100000006,"d":"0.36"},{"v":2.423650120492838,"d":"2.42"},{"v":2.423650120492838,"d":"2.42"},{"v":0.8517764644999999,"d":"0.85"}]
["08045","Garfield","CO",{"v":0.345177957,"d":"0.35"},{"v":2.7013351418639835,"d":"2.70"},{"v":2.701335141863983,"d":"2.70"},{"v":0.897519119,"d":"0.90"}]
["08047","Gilpin","CO",{"v":0.39377115499999993,"d":"0.39"},{"v":2.685948569900042,"d":"2.69"},{"v":2.6859485699000416,"d":"2.69"},{"v":1.0950876315000002,"d":"1.10"}]
["08049","Grand","CO",{"v":0.390552728,"d":"0.39"},{"v":2.8173082355821593,"d":"2.82"},{"v":2.8173082355821597,"d":"2.82"},{"v":0.9971690025000001,"d":"1.00"}]
["08051","Gunnison","CO",{"v":0.360305304,"d":"0.36"},{"v":2.675727481180688,"d":"2.68"},{"v":2.675727481180688,"d":"2.68"},{"v":0.9993224510000003,"d":"1.00"}]
["08053","Hinsdale","CO",{"v":0.402611448,"d":"0.40"},{"v":2.95358707587503,"d":"2.95"},{"v":2.9535870758750296,"d":"2.95"},{"v":1.0827734669999998,"d":"1.08"}]
["08055","Huerfano","CO",{"v":0.3985753759999999,"d":"0.40"},{"v":2.5327089221065746,"d":"2.53"},{"v":2.5327089221065746,"d":"2.53"},{"v":0.8740302235,"d":"0.87"}]
["08057","Jackson","CO",{"v":0.431257967,"d":"0.43"},{"v":2.780711577026697,"d":"2.78"},{"v":2.780711577026697,"d":"2.78"},{"v":0.9864405964999999,"d":"0.99"}]
["08059","Jefferson","CO",{"v":0.257359873,"d":"0.26"},{"v":2.2788445185515753,"d":"2.28"},{"v":2.2788445185515753,"d":"2.28"},{"v":0.784055915,"d":"0.78"}]
["08061","Kiowa","CO",{"v":0.454119474,"d":"0.45"},{"v":2.4506376845810327,"d":"2.45"},{"v":2.4506376845810327,"d":"2.45"},{"v":0.869157076,"d":"0.87"}]
["08063","Kit Carson","CO",{"v":0.405032462,"d":"0.41"},{"v":2.4365483473109104,"d":"2.44"},{"v":2.43654834731091,"d":"2.44"},{"v":0.816571096,"d":"0.82"}]
["08065","Lake","CO",{"v":0.35022899199999996,"d":"0.35"},{"v":2.4670361791043103,"d":"2.47"},{"v":2.4670361791043103,"d":"2.47"},{"v":0.8587891360000001,"d":"0.86"}]
["08067","La Plata","CO",{"v":0.36437572799999995,"d":"0.36"},{"v":2.7761518277719706,"d":"2.78"},{"v":2.7761518277719706,"d":"2.78"},{"v":0.9691865745,"d":"0.97"}]
["08069","Larimer","CO",{"v":0.320145752,"d":"0.32"},{"v":2.5679195061264477,"d":"2.57"},{"v":2.567919506126448,"d":"2.57"},{"v":0.8361742400000001,"d":"0.84"}]
["08071","Las Animas","CO",{"v":0.38410396,"d":"0.38"},{"v":2.4531414725990466,"d":"2.45"},{"v":2.4531414725990466,"d":"2.45"},{"v":0.8187192530000001,"d":"0.82"}]
["08073","Lincoln","CO",{"v":0.45677648,"d":"0.46"},{"v":2.477468425628722,"d":"2.48"},{"v":2.477468425628722,"d":"2.48"},{"v":0.8634683459999999,"d":"0.86"}]
["08075","Logan","CO",{"v":0.3750166750000001,"d":"0.38"},{"v":2.5840278489690545,"d":"2.58"},{"v":2.584027848969055,"d":"2.58"},{"v":0.7949312585000001,"d":"0.79"}]
["08077","Mesa","CO",{"v":0.327772959,"d":"0.33"},{"v":2.6224901792391515,"d":"2.62"},{"v":2.6224901792391515,"d":"2.62"},{"v":0.8447298785,"d":"0.84"}]
["08079","Mineral","CO",{"v":0.40045713899999996,"d":"0.40"},{"v":2.980794939111311,"d":"2.98"},{"v":2.980794939111311,"d":"2.98"},{"v":1.082251934,"d":"1.08"}]
["08081","Moffat","CO",{"v":0.3514835270000001,"d":"0.35"},{"v":2.6836835674546515,"d":"2.68"},{"v":2.6836835674546515,"d":"2.68"},{"v":0.823416142,"d":"0.82"}]
["08083","Montezuma","CO",{"v":0.3843823920000001,"d":"0.38"},{"v":2.777481067410104,"d":"2.78"},{"v":2.777481067410104,"d":"2.78"},{"v":0.9473364925000002,"d":"0.95"}]
["08085","Montrose","CO",{"v":0.358331856,"d":"0.36"},{"v":2.7344264252465518,"d":"2.73"},{"v":2.7344264252465518,"d":"2.73"},{"v":0.9241741450000002,"d":"0.92"}]
["08087","Morgan","CO",{"v":0.36608155,"d":"0.37"},{"v":2.6026890695799763,"d":"2.60"},{"v":2.6026890695799763,"d":"2.60"},{"v":0.7997911864999998,"d":"0.80"}]
["08089","Otero","CO",{"v":0.38455856,"d":"0.38"},{"v":2.3409664285606246,"d":"2.34"},{"v":2.340966428560625,"d":"2.34"},{"v":0.7715731609999997,"d":"0.77"}]
["08091","Ouray","CO",{"v":0.408972802,"d":"0.41"},{"v":2.7628485996316234,"d":"2.76"},{"v":2.7628485996316234,"d":"2.76"},{"v":1.0560958715,"d":"1.06"}]
["08093","Park","CO",{"v":0.424954586,"d":"0.42"},{"v":2.7037030222962795,"d":"2.70"},{"v":2.7037030222962795,"d":"2.70"},{"v":0.9799400340000002,"d":"0.98"}]
["08095","Phillips","CO",{"v":0.4593718869999999,"d":"0.46"},{"v":2.4842759070931115,"d":"2.48"},{"v":2.4842759070931115,"d":"2.48"},{"v":0.8672507070000001,"d":"0.87"}]
["08097","Pitkin","CO",{"v":0.321445508,"d":"0.32"},{"v":2.8395817764642537,"d":"2.84"},{"v":2.8395817764642537,"d":"2.84"},{"v":0.97733772,"d":"0.98"}]
["08099","Prowers","CO",{"v":0.387929358,"d":"0.39"},{"v":2.3614229280112533,"d":"2.36"},{"v":2.3614229280112533,"d":"2.36"},{"v":0.778692616,"d":"0.78"}]
["08101","Pueblo","CO",{"v":0.35652674200000006,"d":"0.36"},{"v":2.365858911620059,"d":"2.37"},{"v":2.365858911620059,"d":"2.37"},{"v":0.7269305620000001,"d":"0.73"}]
["08103","Rio Blanco","CO",{"v":0.410074726,"d":"0.41"},{"v":2.68813344677824,"d":"2.69"},{"v":2.68813344677824,"d":"2.69"},{"v":1.0184102004999998,"d":"1.02"}]
["08105","Rio Grande","CO",{"v":0.36663924,"d":"0.37"},{"v":2.8184591475109144,"d":"2.82"},{"v":2.8184591475109144,"d":"2.82"},{"v":0.9703533074999999,"d":"0.97"}]
["08107","Routt","CO",{"v":0.358720891,"d":"0.36"},{"v":2.8454256081941485,"d":"2.85"},{"v":2.845425608194149,"d":"2.85"},{"v":0.9411858805000001,"d":"0.94"}]
["08109","Saguache","CO",{"v":0.41141713099999994,"d":"0.41"},{"v":2.903972026187223,"d":"2.90"},{"v":2.903972026187223,"d":"2.90"},{"v":1.025986324,"d":"1.03"}]
["08111","San Juan","CO",{"v":0.400852723,"d":"0.40"},{"v":2.78920656409367,"d":"2.79"},{"v":2.7892065640936696,"d":"2.79"},{"v":1.0266284270000001,"d":"1.03"}]
["08113","San Miguel","CO",{"v":0.3844854569999999,"d":"0.38"},{"v":2.676933671076544,"d":"2.68"},{"v":2.676933671076544,"d":"2.68"},{"v":1.016787903,"d":"1.02"}]
["08115","Sedgwick","CO",{"v":0.458754123,"d":"0.46"},{"v":2.4598788141599686,"d":"2.46"},{"v":2.4598788141599686,"d":"2.46"},{"v":0.8721917860000001,"d":"0.87"}]
["08117","Summit","CO",{"v":0.295602033,"d":"0.30"},{"v":2.765976408274812,"d":"2.77"},{"v":2.765976408274812,"d":"2.77"},{"v":0.891415016,"d":"0.89"}]
["08119","Teller","CO",{"v":0.384900965,"d":"0.38"},{"v":2.490955670417277,"d":"2.49"},{"v":2.490955670417277,"d":"2.49"},{"v":0.943081723,"d":"0.94"}]
["08121","Washington","CO",{"v":0.458623921,"d":"0.46"},{"v":2.508071089564401,"d":"2.51"},{"v":2.508071089564401,"d":"2.51"},{"v":0.870927973,"d":"0.87"}]
["08123","Weld","CO",{"v":0.352205097,"d":"0.35"},{"v":2.5220916493179164,"d":"2.52"},{"v":2.5220916493179164,"d":"2.52"},{"v":0.7620808654999999,"d":"0.76"}]
["08125","Yuma","CO",{"v":0.41892873500000005,"d":"0.42"},{"v":2.4542872090730383,"d":"2.45"},{"v":2.4542872090730388,"d":"2.45"},{"v":0.827970883,"d":"0.83"}]
["09001","Fairfield","CT",{"v":0.152900127,"d":"0.15"},{"v":0.7455702311411729,"d":"0.75"},{"v":0.7455702311411729,"d":"0.75"},{"v":0.607470407,"d":"0.61"}]
["09003","Hartford","CT",{"v":0.163516063,"d":"0.16"},{"v":1.0538867770859428,"d":"1.05"},{"v":1.0538867770859426,"d":"1.05"},{"v":0.661780893,"d":"0.66"}]
["09005","Litchfield","CT",{"v":0.238856927,"d":"0.24"},{"v":2.0657520385584554,"d":"2.07"},{"v":2.065752038558455,"d":"2.07"},{"v":0.8863434805,"d":"0.89"}]
["09007","Middlesex","CT",{"v":0.216768284,"d":"0.22"},{"v":1.9291544258033306,"d":"1.93"},{"v":1.9291544258033304,"d":"1.93"},{"v":0.7516379710000001,"d":"0.75"}]
["09009","New Haven","CT",{"v":0.15527996900000002,"d":"0.16"},{"v":0.7324421997927226,"d":"0.73"},{"v":0.7324421997927226,"d":"0.73"},{"v":0.6124229580000001,"d":"0.61"}]
["09011","New London","CT",{"v":0.223504333,"d":"0.22"},{"v":1.9214054068508726,"d":"1.92"},{"v":1.9214054068508726,"d":"1.92"},{"v":0.7475798104999999,"d":"0.75"}]
["09013","Tolland","CT",{"v":0.22870662700000002,"d":"0.23"},{"v":2.0061170821673504,"d":"2.01"},{"v":2.0061170821673504,"d":"2.01"},{"v":0.8468600834999999,"d":"0.85"}]
["09015","Windham","CT",{"v":0.246236454,"d":"0.25"},{"v":1.9923294147752006,"d":"1.99"},{"v":1.9923294147752009,"d":"1.99"},{"v":0.8864766275000001,"d":"0.89"}]
["10001","Kent","DE",{"v":0.325690073,"d":"0.33"},{"v":2.1754565001844273,"d":"2.18"},{"v":2.1754565001844273,"d":"2.18"},{"v":0.728457245,"d":"0.73"}]
["10003","New Castle","DE",{"v":0.23032864,"d":"0.23"},{"v":1.2458621006460349,"d":"1.25"},{"v":1.2458621006460349,"d":"1.25"},{"v":0.628254627,"d":"0.63"}]
["10005","Sussex","DE",{"v":0.341040462,"d":"0.34"},{"v":2.291138423650407,"d":"2.29"},{"v":2.291138423650407,"d":"2.29"},{"v":0.7741145805,"d":"0.77"}]
["11001","District of Columbia","DC",{"v":0.001539593,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.05978040849999999,"d":"0.06"}]
["12001","Alachua","FL",{"v":0.220501306,"d":"0.22"},{"v":1.4138696972837026,"d":"1.41"},{"v":1.4138696972837026,"d":"1.41"},{"v":0.6021850825,"d":"0.60"}]
["12003","Baker","FL",{"v":0.258269397,"d":"0.26"},{"v":1.5434737688000997,"d":"1.54"},{"v":1.5434737688000995,"d":"1.54"},{"v":0.7296453609999999,"d":"0.73"}]
["12005","Bay","FL",{"v":0.22597903199999997,"d":"0.23"},{"v":1.4681908568602862,"d":"1.47"},{"v":1.4681908568602864,"d":"1.47"},{"v":0.546020493,"d":"0.55"}]
["12007","Bradford","FL",{"v":0.271480629,"d":"0.27"},{"v":1.5144418569801947,"d":"1.51"},{"v":1.5144418569801945,"d":"1.51"},{"v":0.676835977,"d":"0.68"}]
["12009","Brevard","FL",{"v":0.22124892899999998,"d":"0.22"},{"v":1.3104650792400703,"d":"1.31"},{"v":1.3104650792400703,"d":"1.31"},{"v":0.44882938349999996,"d":"0.45"}]
["12011","Broward","FL",{"v":0.15334103099999996,"d":"0.15"},{"v":0.4893339605482366,"d":"0.49"},{"v":0.4893339605482366,"d":"0.49"},{"v":0.37970983399999997,"d":"0.38"}]
["12013","Calhoun","FL",{"v":0.274062484,"d":"0.27"},{"v":1.5428668608347673,"d":"1.54"},{"v":1.5428668608347675,"d":"1.54"},{"v":0.7459614505,"d":"0.75"}]
["12015","Charlotte","FL",{"v":0.245805987,"d":"0.25"},{"v":1.368242542157675,"d":"1.37"},{"v":1.3682425421576752,"d":"1.37"},{"v":0.4744002349999999,"d":"0.47"}]
["12017","Citrus","FL",{"v":0.25673005400000004,"d":"0.26"},{"v":1.4334596115433922,"d":"1.43"},{"v":1.4334596115433924,"d":"1.43"},{"v":0.55074531,"d":"0.55"}]
["12019","Clay","FL",{"v":0.227808542,"d":"0.23"},{"v":1.463835940393221,"d":"1.46"},{"v":1.463835940393221,"d":"1.46"},{"v":0.5767057164999999,"d":"0.58"}]
["12021","Collier","FL",{"v":0.223037333,"d":"0.22"},{"v":1.3596710559987442,"d":"1.36"},{"v":1.359671055998744,"d":"1.36"},{"v":0.5349256015,"d":"0.53"}]
["12023","Columbia","FL",{"v":0.263133474,"d":"0.26"},{"v":1.5139464311373938,"d":"1.51"},{"v":1.5139464311373938,"d":"1.51"},{"v":0.6971950320000001,"d":"0.70"}]
["12027","De Soto","FL",{"v":0.267177839,"d":"0.27"},{"v":1.4572170161929756,"d":"1.46"},{"v":1.4572170161929758,"d":"1.46"},{"v":0.594274969,"d":"0.59"}]
["12029","Dixie","FL",{"v":0.284176847,"d":"0.28"},{"v":1.5770223311573661,"d":"1.58"},{"v":1.577022331157366,"d":"1.58"},{"v":0.6831744185,"d":"0.68"}]
["12031","Duval","FL",{"v":0.168598368,"d":"0.17"},{"v":0.882477450703238,"d":"0.88"},{"v":0.882477450703238,"d":"0.88"},{"v":0.476207772,"d":"0.48"}]
["12033","Escambia","FL",{"v":0.21277123499999998,"d":"0.21"},{"v":1.3799655907494863,"d":"1.38"},{"v":1.3799655907494865,"d":"1.38"},{"v":0.5310980945,"d":"0.53"}]
["12035","Flagler","FL",{"v":0.24093237799999997,"d":"0.24"},{"v":1.4546311943215642,"d":"1.45"},{"v":1.4546311943215642,"d":"1.45"},{"v":0.5396430600000001,"d":"0.54"}]
["12037","Franklin","FL",{"v":0.2931324129999999,"d":"0.29"},{"v":1.505963164948819,"d":"1.51"},{"v":1.505963164948819,"d":"1.51"},{"v":0.5904906125,"d":"0.59"}]
["12039","Gadsden","FL",{"v":0.2667600459999999,"d":"0.27"},{"v":1.5090803267363937,"d":"1.51"},{"v":1.5090803267363935,"d":"1.51"},{"v":0.723822813,"d":"0.72"}]
["12041","Gilchrist","FL",{"v":0.2937765520000001,"d":"0.29"},{"v":1.5764576273635065,"d":"1.58"},{"v":1.5764576273635067,"d":"1.58"},{"v":0.658519019,"d":"0.66"}]
["12043","Glades","FL",{"v":0.308632596,"d":"0.31"},{"v":1.4814397177785892,"d":"1.48"},{"v":1.4814397177785894,"d":"1.48"},{"v":0.566340697,"d":"0.57"}]
["12045","Gulf","FL",{"v":0.291283808,"d":"0.29"},{"v":1.4768297117065665,"d":"1.48"},{"v":1.4768297117065665,"d":"1.48"},{"v":0.6762336840000001,"d":"0.68"}]
["12047","Hamilton","FL",{"v":0.280832553,"d":"0.28"},{"v":1.511564836017591,"d":"1.51"},{"v":1.511564836017591,"d":"1.51"},{"v":0.6971995544999999,"d":"0.70"}]
["12049","Hardee","FL",{"v":0.268261912,"d":"0.27"},{"v":1.4552416725657658,"d":"1.46"},{"v":1.4552416725657658,"d":"1.46"},{"v":0.6126654914999999,"d":"0.61"}]
["12051","Hendry","FL",{"v":0.2738385,"d":"0.27"},{"v":1.4454891903871128,"d":"1.45"},{"v":1.4454891903871128,"d":"1.45"},{"v":0.563178917,"d":"0.56"}]
["12053","Hernando","FL",{"v":0.23386091299999998,"d":"0.23"},{"v":1.4056426282164107,"d":"1.41"},{"v":1.4056426282164107,"d":"1.41"},{"v":0.5436244494999999,"d":"0.54"}]
["12055","Highlands","FL",{"v":0.259972322,"d":"0.26"},{"v":1.4200908902333524,"d":"1.42"},{"v":1.4200908902333524,"d":"1.42"},{"v":0.5429253585,"d":"0.54"}]
["12057","Hillsborough","FL",{"v":0.168527783,"d":"0.17"},{"v":0.7159255420086795,"d":"0.72"},{"v":0.7159255420086795,"d":"0.72"},{"v":0.449216071,"d":"0.45"}]
["12059","Holmes","FL",{"v":0.28404583200000005,"d":"0.28"},{"v":1.5384195257039288,"d":"1.54"},{"v":1.538419525703929,"d":"1.54"},{"v":0.722613988,"d":"0.72"}]
["12061","Indian River","FL",{"v":0.227089383,"d":"0.23"},{"v":1.3819704543792248,"d":"1.38"},{"v":1.3819704543792248,"d":"1.38"},{"v":0.5112383375,"d":"0.51"}]
["12063","Jackson","FL",{"v":0.288037916,"d":"0.29"},{"v":1.519913087475567,"d":"1.52"},{"v":1.519913087475567,"d":"1.52"},{"v":0.6713619554999998,"d":"0.67"}]
["12065","Jefferson","FL",{"v":0.29056376000000006,"d":"0.29"},{"v":1.562970257316414,"d":"1.56"},{"v":1.562970257316414,"d":"1.56"},{"v":0.7561658075,"d":"0.76"}]
["12067","Lafayette","FL",{"v":0.290015477,"d":"0.29"},{"v":1.5828006126123528,"d":"1.58"},{"v":1.5828006126123528,"d":"1.58"},{"v":0.749967296,"d":"0.75"}]
["12069","Lake","FL",{"v":0.234541865,"d":"0.23"},{"v":1.3950108693095633,"d":"1.40"},{"v":1.3950108693095633,"d":"1.40"},{"v":0.5343330614999999,"d":"0.53"}]
["12071","Lee","FL",{"v":0.20266925100000002,"d":"0.20"},{"v":1.1659656770698354,"d":"1.17"},{"v":1.1659656770698357,"d":"1.17"},{"v":0.4361932415,"d":"0.44"}]
["12073","Leon","FL",{"v":0.205632101,"d":"0.21"},{"v":1.4231116912432662,"d":"1.42"},{"v":1.4231116912432662,"d":"1.42"},{"v":0.6291807899999999,"d":"0.63"}]
["12075","Levy","FL",{"v":0.295113565,"d":"0.30"},{"v":1.5678120187427418,"d":"1.57"},{"v":1.5678120187427418,"d":"1.57"},{"v":0.6548239385,"d":"0.65"}]
["12077","Liberty","FL",{"v":0.279907416,"d":"0.28"},{"v":1.6177134506427007,"d":"1.62"},{"v":1.6177134506427011,"d":"1.62"},{"v":0.8165148745,"d":"0.82"}]
["12079","Madison","FL",{"v":0.282872634,"d":"0.28"},{"v":1.5326516060827375,"d":"1.53"},{"v":1.5326516060827375,"d":"1.53"},{"v":0.7114493925,"d":"0.71"}]
["12081","Manatee","FL",{"v":0.22537502699999998,"d":"0.23"},{"v":1.3678310424118394,"d":"1.37"},{"v":1.3678310424118396,"d":"1.37"},{"v":0.46666166600000003,"d":"0.47"}]
["12083","Marion","FL",{"v":0.24975615,"d":"0.25"},{"v":1.4163913150345606,"d":"1.42"},{"v":1.4163913150345606,"d":"1.42"},{"v":0.5794511765000001,"d":"0.58"}]
["12085","Martin","FL",{"v":0.243416177,"d":"0.24"},{"v":1.3751353954576708,"d":"1.38"},{"v":1.3751353954576708,"d":"1.38"},{"v":0.47277392149999997,"d":"0.47"}]
["12086","Miami-Dade","FL",{"v":0.159640662,"d":"0.16"},{"v":0.8502482624727682,"d":"0.85"},{"v":0.8502482624727682,"d":"0.85"},{"v":0.3861912575,"d":"0.39"}]
["12087","Monroe","FL",{"v":0.267399949,"d":"0.27"},{"v":1.3707502000591858,"d":"1.37"},{"v":1.3707502000591856,"d":"1.37"},{"v":0.45588577,"d":"0.46"}]
["12089","Nassau","FL",{"v":0.259774003,"d":"0.26"},{"v":1.484745643999032,"d":"1.48"},{"v":1.4847456439990319,"d":"1.48"},{"v":0.629714839,"d":"0.63"}]
["12091","Okaloosa","FL",{"v":0.228624996,"d":"0.23"},{"v":1.420371030794363,"d":"1.42"},{"v":1.4203710307943629,"d":"1.42"},{"v":0.560699237,"d":"0.56"}]
["12093","Okeechobee","FL",{"v":0.277055837,"d":"0.28"},{"v":1.4608071631205684,"d":"1.46"},{"v":1.4608071631205681,"d":"1.46"},{"v":0.5218555364999999,"d":"0.52"}]
["12095","Orange","FL",{"v":0.15922500200000003,"d":"0.16"},{"v":0.7075536365960039,"d":"0.71"},{"v":0.7075536365960038,"d":"0.71"},{"v":0.448458302,"d":"0.45"}]
["12097","Osceola","FL",{"v":0.243497327,"d":"0.24"},{"v":1.4073323316543718,"d":"1.41"},{"v":1.4073323316543718,"d":"1.41"},{"v":0.4866821665,"d":"0.49"}]
["12099","Palm Beach","FL",{"v":0.212830099,"d":"0.21"},{"v":1.2500102486736946,"d":"1.25"},{"v":1.2500102486736946,"d":"1.25"},{"v":0.41802302500000005,"d":"0.42"}]
["12101","Pasco","FL",{"v":0.20796929499999997,"d":"0.21"},{"v":1.3281019256889448,"d":"1.33"},{"v":1.3281019256889448,"d":"1.33"},{"v":0.509551516,"d":"0.51"}]
["12103","Pinellas","FL",{"v":0.085290444,"d":"0.09"},{"v":7.0960266696841245E-5,"d":"0.00"},{"v":7.0960266696841245E-5,"d":"0.00"},{"v":0.318966528,"d":"0.32"}]
["12105","Polk","FL",{"v":0.23147969000000002,"d":"0.23"},{"v":1.38669269372967,"d":"1.39"},{"v":1.3866926937296695,"d":"1.39"},{"v":0.5259309374999999,"d":"0.53"}]
["12107","Putnam","FL",{"v":0.26399364200000003,"d":"0.26"},{"v":1.519215940252309,"d":"1.52"},{"v":1.5192159402523093,"d":"1.52"},{"v":0.6316360424999999,"d":"0.63"}]
["12109","St Johns","FL",{"v":0.23676500799999997,"d":"0.24"},{"v":1.4404637531506417,"d":"1.44"},{"v":1.4404637531506417,"d":"1.44"},{"v":0.5385813075,"d":"0.54"}]
["12111","St Lucie","FL",{"v":0.21501677200000002,"d":"0.22"},{"v":1.3413223417348705,"d":"1.34"},{"v":1.3413223417348705,"d":"1.34"},{"v":0.4956988055,"d":"0.50"}]
["12113","Santa Rosa","FL",{"v":0.24407804699999996,"d":"0.24"},{"v":1.466413845325359,"d":"1.47"},{"v":1.466413845325359,"d":"1.47"},{"v":0.5834583635,"d":"0.58"}]
["12115","Sarasota","FL",{"v":0.209343224,"d":"0.21"},{"v":1.2189718976944524,"d":"1.22"},{"v":1.2189718976944521,"d":"1.22"},{"v":0.44549692700000004,"d":"0.45"}]
["12117","Seminole","FL",{"v":0.161094602,"d":"0.16"},{"v":0.635900354362081,"d":"0.64"},{"v":0.6359003543620811,"d":"0.64"},{"v":0.4618741794999999,"d":"0.46"}]
["12119","Sumter","FL",{"v":0.248577116,"d":"0.25"},{"v":1.364355788575946,"d":"1.36"},{"v":1.364355788575946,"d":"1.36"},{"v":0.559603603,"d":"0.56"}]
["12121","Suwannee","FL",{"v":0.284666729,"d":"0.28"},{"v":1.57331000628275,"d":"1.57"},{"v":1.5733100062827499,"d":"1.57"},{"v":0.6503219365,"d":"0.65"}]
["12123","Taylor","FL",{"v":0.279496778,"d":"0.28"},{"v":1.4950553758166554,"d":"1.50"},{"v":1.4950553758166556,"d":"1.50"},{"v":0.665711845,"d":"0.67"}]
["12125","Union","FL",{"v":0.27190475399999997,"d":"0.27"},{"v":1.5468020941170555,"d":"1.55"},{"v":1.546802094117056,"d":"1.55"},{"v":0.7084406119999999,"d":"0.71"}]
["12127","Volusia","FL",{"v":0.219003264,"d":"0.22"},{"v":1.3664338200290722,"d":"1.37"},{"v":1.3664338200290722,"d":"1.37"},{"v":0.5089945604999998,"d":"0.51"}]
["12129","Wakulla","FL",{"v":0.273710581,"d":"0.27"},{"v":1.5471534627375618,"d":"1.55"},{"v":1.5471534627375618,"d":"1.55"},{"v":0.7178684780000001,"d":"0.72"}]
["12131","Walton","FL",{"v":0.264297715,"d":"0.26"},{"v":1.494781321744299,"d":"1.49"},{"v":1.494781321744299,"d":"1.49"},{"v":0.6412648609999999,"d":"0.64"}]
["12133","Washington","FL",{"v":0.280825811,"d":"0.28"},{"v":1.555805166330526,"d":"1.56"},{"v":1.555805166330526,"d":"1.56"},{"v":0.7129632545,"d":"0.71"}]
["13001","Appling","GA",{"v":0.247458283,"d":"0.25"},{"v":1.3800537904997423,"d":"1.38"},{"v":1.3800537904997423,"d":"1.38"},{"v":0.6244326880000001,"d":"0.62"}]
["13003","Atkinson","GA",{"v":0.260594658,"d":"0.26"},{"v":1.4562009992704443,"d":"1.46"},{"v":1.456200999270444,"d":"1.46"},{"v":0.6637718404999999,"d":"0.66"}]
["13005","Bacon","GA",{"v":0.252988438,"d":"0.25"},{"v":1.3741178804066534,"d":"1.37"},{"v":1.374117880406653,"d":"1.37"},{"v":0.603467452,"d":"0.60"}]
["13007","Baker","GA",{"v":0.276330648,"d":"0.28"},{"v":1.402259857530967,"d":"1.40"},{"v":1.402259857530967,"d":"1.40"},{"v":0.6084040924999999,"d":"0.61"}]
["13009","Baldwin","GA",{"v":0.204309716,"d":"0.20"},{"v":1.351359230256149,"d":"1.35"},{"v":1.3513592302561492,"d":"1.35"},{"v":0.6370170625,"d":"0.64"}]
["13011","Banks","GA",{"v":0.2516920080000001,"d":"0.25"},{"v":1.4972646673146235,"d":"1.50"},{"v":1.4972646673146235,"d":"1.50"},{"v":0.678895051,"d":"0.68"}]
["13013","Barrow","GA",{"v":0.19527494699999998,"d":"0.20"},{"v":1.3984767217826246,"d":"1.40"},{"v":1.3984767217826246,"d":"1.40"},{"v":0.560140399,"d":"0.56"}]
["13015","Bartow","GA",{"v":0.207252397,"d":"0.21"},{"v":1.4161608214217696,"d":"1.42"},{"v":1.4161608214217694,"d":"1.42"},{"v":0.60815721,"d":"0.61"}]
["13017","Ben Hill","GA",{"v":0.223371487,"d":"0.22"},{"v":1.3544139744728463,"d":"1.35"},{"v":1.354413974472846,"d":"1.35"},{"v":0.588392607,"d":"0.59"}]
["13019","Berrien","GA",{"v":0.250563083,"d":"0.25"},{"v":1.4027639656375506,"d":"1.40"},{"v":1.4027639656375506,"d":"1.40"},{"v":0.632621101,"d":"0.63"}]
["13021","Bibb","GA",{"v":0.172862415,"d":"0.17"},{"v":1.1995883353708392,"d":"1.20"},{"v":1.1995883353708392,"d":"1.20"},{"v":0.5551269695,"d":"0.56"}]
["13023","Bleckley","GA",{"v":0.239423987,"d":"0.24"},{"v":1.386435119914823,"d":"1.39"},{"v":1.386435119914823,"d":"1.39"},{"v":0.600298711,"d":"0.60"}]
["13025","Brantley","GA",{"v":0.253994391,"d":"0.25"},{"v":1.4547803470953125,"d":"1.45"},{"v":1.4547803470953125,"d":"1.45"},{"v":0.68475914,"d":"0.68"}]
["13027","Brooks","GA",{"v":0.25544277000000004,"d":"0.26"},{"v":1.3899870577617088,"d":"1.39"},{"v":1.3899870577617088,"d":"1.39"},{"v":0.602296409,"d":"0.60"}]
["13029","Bryan","GA",{"v":0.23367321799999996,"d":"0.23"},{"v":1.3428195741982079,"d":"1.34"},{"v":1.3428195741982076,"d":"1.34"},{"v":0.641263086,"d":"0.64"}]
["13031","Bulloch","GA",{"v":0.22405234800000004,"d":"0.22"},{"v":1.3494277773739614,"d":"1.35"},{"v":1.3494277773739614,"d":"1.35"},{"v":0.5993467200000001,"d":"0.60"}]
["13033","Burke","GA",{"v":0.254663678,"d":"0.25"},{"v":1.402729529401223,"d":"1.40"},{"v":1.4027295294012228,"d":"1.40"},{"v":0.6276491474999999,"d":"0.63"}]
["13035","Butts","GA",{"v":0.238579844,"d":"0.24"},{"v":1.3779538108787763,"d":"1.38"},{"v":1.377953810878776,"d":"1.38"},{"v":0.6734926945000002,"d":"0.67"}]
["13037","Calhoun","GA",{"v":0.271007718,"d":"0.27"},{"v":1.3709646792996208,"d":"1.37"},{"v":1.3709646792996208,"d":"1.37"},{"v":0.62633453,"d":"0.63"}]
["13039","Camden","GA",{"v":0.233748274,"d":"0.23"},{"v":1.3338879729289963,"d":"1.33"},{"v":1.333887972928996,"d":"1.33"},{"v":0.5608337805,"d":"0.56"}]
["13043","Candler","GA",{"v":0.24622145599999998,"d":"0.25"},{"v":1.4291144122623824,"d":"1.43"},{"v":1.4291144122623824,"d":"1.43"},{"v":0.6041178989999999,"d":"0.60"}]
["13045","Carroll","GA",{"v":0.21256722600000003,"d":"0.21"},{"v":1.347020490876224,"d":"1.35"},{"v":1.347020490876224,"d":"1.35"},{"v":0.616477777,"d":"0.62"}]
["13047","Catoosa","GA",{"v":0.194878899,"d":"0.19"},{"v":1.405674079182204,"d":"1.41"},{"v":1.4056740791822038,"d":"1.41"},{"v":0.571149986,"d":"0.57"}]
["13049","Charlton","GA",{"v":0.23299403599999996,"d":"0.23"},{"v":1.4186376870183457,"d":"1.42"},{"v":1.4186376870183457,"d":"1.42"},{"v":0.6672090919999999,"d":"0.67"}]
["13051","Chatham","GA",{"v":0.189328013,"d":"0.19"},{"v":1.1698630692490408,"d":"1.17"},{"v":1.1698630692490406,"d":"1.17"},{"v":0.41472140799999996,"d":"0.41"}]
["13053","Chattahoochee","GA",{"v":0.251580106,"d":"0.25"},{"v":1.3758018664045206,"d":"1.38"},{"v":1.3758018664045206,"d":"1.38"},{"v":0.656244213,"d":"0.66"}]
["13055","Chattooga","GA",{"v":0.22474206800000002,"d":"0.22"},{"v":1.4404910306453282,"d":"1.44"},{"v":1.4404910306453282,"d":"1.44"},{"v":0.6905319565,"d":"0.69"}]
["13057","Cherokee","GA",{"v":0.17579985,"d":"0.18"},{"v":1.2772274858093209,"d":"1.28"},{"v":1.2772274858093207,"d":"1.28"},{"v":0.6068225995000001,"d":"0.61"}]
["13059","Clarke","GA",{"v":0.14366790800000004,"d":"0.14"},{"v":1.0236391734588504,"d":"1.02"},{"v":1.0236391734588506,"d":"1.02"},{"v":0.5343181004999998,"d":"0.53"}]
["13061","Clay","GA",{"v":0.26683989,"d":"0.27"},{"v":1.4075192274261457,"d":"1.41"},{"v":1.4075192274261457,"d":"1.41"},{"v":0.637965519,"d":"0.64"}]
["13063","Clayton","GA",{"v":0.111583123,"d":"0.11"},{"v":0.2435870580050863,"d":"0.24"},{"v":0.2435870580050863,"d":"0.24"},{"v":0.4572754895,"d":"0.46"}]
["13065","Clinch","GA",{"v":0.23533220099999996,"d":"0.24"},{"v":1.4028002042656829,"d":"1.40"},{"v":1.4028002042656829,"d":"1.40"},{"v":0.668347361,"d":"0.67"}]
["13067","Cobb","GA",{"v":0.10162582999999999,"d":"0.10"},{"v":0.058110171386160335,"d":"0.06"},{"v":0.058110171386160335,"d":"0.06"},{"v":0.4719506215,"d":"0.47"}]
["13069","Coffee","GA",{"v":0.243469429,"d":"0.24"},{"v":1.3820572475940844,"d":"1.38"},{"v":1.3820572475940844,"d":"1.38"},{"v":0.6038976465,"d":"0.60"}]
["13071","Colquitt","GA",{"v":0.245299166,"d":"0.25"},{"v":1.4009323146560313,"d":"1.40"},{"v":1.4009323146560315,"d":"1.40"},{"v":0.5710389589999999,"d":"0.57"}]
["13073","Columbia","GA",{"v":0.19096736900000003,"d":"0.19"},{"v":1.287986677972999,"d":"1.29"},{"v":1.2879866779729991,"d":"1.29"},{"v":0.559238149,"d":"0.56"}]
["13075","Cook","GA",{"v":0.24662969200000004,"d":"0.25"},{"v":1.4039331261592927,"d":"1.40"},{"v":1.4039331261592927,"d":"1.40"},{"v":0.5812057605000001,"d":"0.58"}]
["13077","Coweta","GA",{"v":0.20032222200000002,"d":"0.20"},{"v":1.2890568988220434,"d":"1.29"},{"v":1.2890568988220432,"d":"1.29"},{"v":0.6210442249999999,"d":"0.62"}]
["13079","Crawford","GA",{"v":0.256684302,"d":"0.26"},{"v":1.4586307859942649,"d":"1.46"},{"v":1.4586307859942649,"d":"1.46"},{"v":0.6854991245000001,"d":"0.69"}]
["13081","Crisp","GA",{"v":0.236104882,"d":"0.24"},{"v":1.3472962094457712,"d":"1.35"},{"v":1.3472962094457712,"d":"1.35"},{"v":0.554843095,"d":"0.55"}]
["13083","Dade","GA",{"v":0.23211981600000003,"d":"0.23"},{"v":1.5063635720266189,"d":"1.51"},{"v":1.5063635720266189,"d":"1.51"},{"v":0.7036628675,"d":"0.70"}]
["13085","Dawson","GA",{"v":0.232259584,"d":"0.23"},{"v":1.465490556683288,"d":"1.47"},{"v":1.465490556683288,"d":"1.47"},{"v":0.7508477815000001,"d":"0.75"}]
["13087","Decatur","GA",{"v":0.24847277799999998,"d":"0.25"},{"v":1.3565684019463384,"d":"1.36"},{"v":1.3565684019463382,"d":"1.36"},{"v":0.5795801859999999,"d":"0.58"}]
["13089","De Kalb","GA",{"v":0.081668747,"d":"0.08"},{"v":0.007139686986556731,"d":"0.01"},{"v":0.007139686986556731,"d":"0.01"},{"v":0.46046249149999996,"d":"0.46"}]
["13091","Dodge","GA",{"v":0.243654346,"d":"0.24"},{"v":1.4174254234221053,"d":"1.42"},{"v":1.4174254234221053,"d":"1.42"},{"v":0.6379779485,"d":"0.64"}]
["13093","Dooly","GA",{"v":0.254914476,"d":"0.25"},{"v":1.3740136715634432,"d":"1.37"},{"v":1.3740136715634432,"d":"1.37"},{"v":0.5642215649999999,"d":"0.56"}]
["13095","Dougherty","GA",{"v":0.19985007299999996,"d":"0.20"},{"v":1.2411124143291743,"d":"1.24"},{"v":1.2411124143291743,"d":"1.24"},{"v":0.5729025795000001,"d":"0.57"}]
["13097","Douglas","GA",{"v":0.168071177,"d":"0.17"},{"v":1.2010338170295218,"d":"1.20"},{"v":1.2010338170295218,"d":"1.20"},{"v":0.5806893645000001,"d":"0.58"}]
["13099","Early","GA",{"v":0.25790428,"d":"0.26"},{"v":1.372371438841256,"d":"1.37"},{"v":1.3723714388412562,"d":"1.37"},{"v":0.5940536040000001,"d":"0.59"}]
["13101","Echols","GA",{"v":0.248640768,"d":"0.25"},{"v":1.4687840826248288,"d":"1.47"},{"v":1.4687840826248286,"d":"1.47"},{"v":0.7192884254999998,"d":"0.72"}]
["13103","Effingham","GA",{"v":0.232912217,"d":"0.23"},{"v":1.4050091146811596,"d":"1.41"},{"v":1.4050091146811596,"d":"1.41"},{"v":0.6703823560000001,"d":"0.67"}]
["13105","Elbert","GA",{"v":0.23679813200000002,"d":"0.24"},{"v":1.4241415668314956,"d":"1.42"},{"v":1.4241415668314956,"d":"1.42"},{"v":0.6422194565000002,"d":"0.64"}]
["13107","Emanuel","GA",{"v":0.24501854499999998,"d":"0.25"},{"v":1.3827500603763951,"d":"1.38"},{"v":1.3827500603763951,"d":"1.38"},{"v":0.644691354,"d":"0.64"}]
["13109","Evans","GA",{"v":0.239507356,"d":"0.24"},{"v":1.3583941856376416,"d":"1.36"},{"v":1.3583941856376414,"d":"1.36"},{"v":0.6137377,"d":"0.61"}]
["13111","Fannin","GA",{"v":0.24274811,"d":"0.24"},{"v":1.5200639092591057,"d":"1.52"},{"v":1.5200639092591057,"d":"1.52"},{"v":0.8031304810000001,"d":"0.80"}]
["13113","Fayette","GA",{"v":0.1804682,"d":"0.18"},{"v":1.2071014182998636,"d":"1.21"},{"v":1.2071014182998634,"d":"1.21"},{"v":0.5748085755,"d":"0.57"}]
["13115","Floyd","GA",{"v":0.20832758700000004,"d":"0.21"},{"v":1.3393736151331346,"d":"1.34"},{"v":1.3393736151331346,"d":"1.34"},{"v":0.6228037125000001,"d":"0.62"}]
["13117","Forsyth","GA",{"v":0.16353056199999996,"d":"0.16"},{"v":1.1525139538585043,"d":"1.15"},{"v":1.152513953858504,"d":"1.15"},{"v":0.5089719764999999,"d":"0.51"}]
["13119","Franklin","GA",{"v":0.253931909,"d":"0.25"},{"v":1.465964639552543,"d":"1.47"},{"v":1.465964639552543,"d":"1.47"},{"v":0.634156657,"d":"0.63"}]
["13121","Fulton","GA",{"v":0.100519615,"d":"0.10"},{"v":0.10826795928413945,"d":"0.11"},{"v":0.10826795928413946,"d":"0.11"},{"v":0.49337647849999994,"d":"0.49"}]
["13123","Gilmer","GA",{"v":0.23226087199999998,"d":"0.23"},{"v":1.5216332852567929,"d":"1.52"},{"v":1.5216332852567929,"d":"1.52"},{"v":0.8018932080000001,"d":"0.80"}]
["13125","Glascock","GA",{"v":0.258365193,"d":"0.26"},{"v":1.4323846384835208,"d":"1.43"},{"v":1.4323846384835206,"d":"1.43"},{"v":0.6924186149999999,"d":"0.69"}]
["13127","Glynn","GA",{"v":0.22135617799999996,"d":"0.22"},{"v":1.3083682975878304,"d":"1.31"},{"v":1.3083682975878304,"d":"1.31"},{"v":0.48983374799999996,"d":"0.49"}]
["13129","Gordon","GA",{"v":0.219196695,"d":"0.22"},{"v":1.4389216010758175,"d":"1.44"},{"v":1.4389216010758172,"d":"1.44"},{"v":0.6263010729999999,"d":"0.63"}]
["13131","Grady","GA",{"v":0.243945037,"d":"0.24"},{"v":1.3765777348114832,"d":"1.38"},{"v":1.376577734811483,"d":"1.38"},{"v":0.6046585590000001,"d":"0.60"}]
["13133","Greene","GA",{"v":0.25101890699999996,"d":"0.25"},{"v":1.402858186574236,"d":"1.40"},{"v":1.4028581865742358,"d":"1.40"},{"v":0.700593497,"d":"0.70"}]
["13135","Gwinnett","GA",{"v":0.107233167,"d":"0.11"},{"v":0.2254576300281638,"d":"0.23"},{"v":0.22545763002816374,"d":"0.23"},{"v":0.4527728325,"d":"0.45"}]
["13137","Habersham","GA",{"v":0.22283352699999995,"d":"0.22"},{"v":1.4569892354656822,"d":"1.46"},{"v":1.4569892354656822,"d":"1.46"},{"v":0.6864538535000001,"d":"0.69"}]
["13139","Hall","GA",{"v":0.18592289000000004,"d":"0.19"},{"v":1.3831985049598237,"d":"1.38"},{"v":1.3831985049598239,"d":"1.38"},{"v":0.5531891889999999,"d":"0.55"}]
["13141","Hancock","GA",{"v":0.232951823,"d":"0.23"},{"v":1.4488683217168263,"d":"1.45"},{"v":1.4488683217168263,"d":"1.45"},{"v":0.7092240584999999,"d":"0.71"}]
["13143","Haralson","GA",{"v":0.236160328,"d":"0.24"},{"v":1.3840858095533801,"d":"1.38"},{"v":1.3840858095533801,"d":"1.38"},{"v":0.7012898325,"d":"0.70"}]
["13145","Harris","GA",{"v":0.25080944,"d":"0.25"},{"v":1.416544054957331,"d":"1.42"},{"v":1.4165440549573307,"d":"1.42"},{"v":0.7311805665000001,"d":"0.73"}]
["13147","Hart","GA",{"v":0.251558317,"d":"0.25"},{"v":1.4358833018557298,"d":"1.44"},{"v":1.4358833018557298,"d":"1.44"},{"v":0.582456369,"d":"0.58"}]
["13149","Heard","GA",{"v":0.25567100400000004,"d":"0.26"},{"v":1.456318453327008,"d":"1.46"},{"v":1.456318453327008,"d":"1.46"},{"v":0.7138783860000001,"d":"0.71"}]
["13151","Henry","GA",{"v":0.173321345,"d":"0.17"},{"v":1.2224846919581638,"d":"1.22"},{"v":1.2224846919581638,"d":"1.22"},{"v":0.5347335310000001,"d":"0.53"}]
["13153","Houston","GA",{"v":0.187913531,"d":"0.19"},{"v":1.3386657348228261,"d":"1.34"},{"v":1.3386657348228264,"d":"1.34"},{"v":0.549849141,"d":"0.55"}]
["13155","Irwin","GA",{"v":0.255717587,"d":"0.26"},{"v":1.356774271471387,"d":"1.36"},{"v":1.356774271471387,"d":"1.36"},{"v":0.5949303075000001,"d":"0.59"}]
["13157","Jackson","GA",{"v":0.226654806,"d":"0.23"},{"v":1.4505239004174642,"d":"1.45"},{"v":1.4505239004174642,"d":"1.45"},{"v":0.617726186,"d":"0.62"}]
["13159","Jasper","GA",{"v":0.24411083,"d":"0.24"},{"v":1.4017195317472428,"d":"1.40"},{"v":1.4017195317472428,"d":"1.40"},{"v":0.7135527,"d":"0.71"}]
["13161","Jeff Davis","GA",{"v":0.245373017,"d":"0.25"},{"v":1.387457839728563,"d":"1.39"},{"v":1.387457839728563,"d":"1.39"},{"v":0.6252703970000001,"d":"0.63"}]
["13163","Jefferson","GA",{"v":0.255586111,"d":"0.26"},{"v":1.3679405149249029,"d":"1.37"},{"v":1.3679405149249027,"d":"1.37"},{"v":0.6434805695,"d":"0.64"}]
["13165","Jenkins","GA",{"v":0.243553346,"d":"0.24"},{"v":1.39431466915653,"d":"1.39"},{"v":1.3943146691565298,"d":"1.39"},{"v":0.6277720665,"d":"0.63"}]
["13167","Johnson","GA",{"v":0.247798547,"d":"0.25"},{"v":1.4017300596463778,"d":"1.40"},{"v":1.4017300596463778,"d":"1.40"},{"v":0.6530118945,"d":"0.65"}]
["13169","Jones","GA",{"v":0.23347581,"d":"0.23"},{"v":1.3765744112675875,"d":"1.38"},{"v":1.3765744112675873,"d":"1.38"},{"v":0.7011313410000001,"d":"0.70"}]
["13171","Lamar","GA",{"v":0.23324470900000002,"d":"0.23"},{"v":1.3719676256370887,"d":"1.37"},{"v":1.3719676256370887,"d":"1.37"},{"v":0.650374755,"d":"0.65"}]
["13173","Lanier","GA",{"v":0.24164272899999997,"d":"0.24"},{"v":1.3857713319568778,"d":"1.39"},{"v":1.3857713319568778,"d":"1.39"},{"v":0.6644262735,"d":"0.66"}]
["13175","Laurens","GA",{"v":0.233556325,"d":"0.23"},{"v":1.4159607565888694,"d":"1.42"},{"v":1.4159607565888694,"d":"1.42"},{"v":0.6308720640000001,"d":"0.63"}]
["13177","Lee","GA",{"v":0.23115939,"d":"0.23"},{"v":1.3498826145904352,"d":"1.35"},{"v":1.3498826145904355,"d":"1.35"},{"v":0.562857685,"d":"0.56"}]
["13179","Liberty","GA",{"v":0.219497512,"d":"0.22"},{"v":1.324358426450347,"d":"1.32"},{"v":1.324358426450347,"d":"1.32"},{"v":0.586612008,"d":"0.59"}]
["13181","Lincoln","GA",{"v":0.260816337,"d":"0.26"},{"v":1.5110174851002436,"d":"1.51"},{"v":1.5110174851002434,"d":"1.51"},{"v":0.6610209585000001,"d":"0.66"}]
["13183","Long","GA",{"v":0.24060274600000003,"d":"0.24"},{"v":1.4457112458593693,"d":"1.45"},{"v":1.4457112458593695,"d":"1.45"},{"v":0.68274603,"d":"0.68"}]
["13185","Lowndes","GA",{"v":0.206654115,"d":"0.21"},{"v":1.3331964860283445,"d":"1.33"},{"v":1.3331964860283445,"d":"1.33"},{"v":0.580599831,"d":"0.58"}]
["13187","Lumpkin","GA",{"v":0.23493890499999998,"d":"0.23"},{"v":1.5186694185432383,"d":"1.52"},{"v":1.5186694185432383,"d":"1.52"},{"v":0.7728411464999999,"d":"0.77"}]
["13189","McDuffie","GA",{"v":0.231195085,"d":"0.23"},{"v":1.3441298259035481,"d":"1.34"},{"v":1.3441298259035481,"d":"1.34"},{"v":0.6535272515,"d":"0.65"}]
["13191","McIntosh","GA",{"v":0.264733318,"d":"0.26"},{"v":1.3906174820985913,"d":"1.39"},{"v":1.3906174820985915,"d":"1.39"},{"v":0.5648376745,"d":"0.56"}]
["13193","Macon","GA",{"v":0.237916479,"d":"0.24"},{"v":1.4205486524051465,"d":"1.42"},{"v":1.4205486524051465,"d":"1.42"},{"v":0.6263563695000001,"d":"0.63"}]
["13195","Madison","GA",{"v":0.253849324,"d":"0.25"},{"v":1.476165503316799,"d":"1.48"},{"v":1.4761655033167993,"d":"1.48"},{"v":0.6443902739999999,"d":"0.64"}]
["13197","Marion","GA",{"v":0.259719645,"d":"0.26"},{"v":1.4873976605133574,"d":"1.49"},{"v":1.4873976605133574,"d":"1.49"},{"v":0.670045431,"d":"0.67"}]
["13199","Meriwether","GA",{"v":0.24429806799999998,"d":"0.24"},{"v":1.441985932919522,"d":"1.44"},{"v":1.441985932919522,"d":"1.44"},{"v":0.701306041,"d":"0.70"}]
["13201","Miller","GA",{"v":0.29117753299999993,"d":"0.29"},{"v":1.3730595265941121,"d":"1.37"},{"v":1.3730595265941123,"d":"1.37"},{"v":0.5644858235,"d":"0.56"}]
["13205","Mitchell","GA",{"v":0.24753245699999996,"d":"0.25"},{"v":1.3700222125222654,"d":"1.37"},{"v":1.3700222125222654,"d":"1.37"},{"v":0.5749055399999999,"d":"0.57"}]
["13207","Monroe","GA",{"v":0.24139316500000002,"d":"0.24"},{"v":1.3823967444622194,"d":"1.38"},{"v":1.3823967444622194,"d":"1.38"},{"v":0.7031121785,"d":"0.70"}]
["13209","Montgomery","GA",{"v":0.260985338,"d":"0.26"},{"v":1.449274922221407,"d":"1.45"},{"v":1.4492749222214072,"d":"1.45"},{"v":0.6710698,"d":"0.67"}]
["13211","Morgan","GA",{"v":0.24843900299999996,"d":"0.25"},{"v":1.375452329030817,"d":"1.38"},{"v":1.375452329030817,"d":"1.38"},{"v":0.6562770415,"d":"0.66"}]
["13213","Murray","GA",{"v":0.22566867199999996,"d":"0.23"},{"v":1.5321852036030066,"d":"1.53"},{"v":1.5321852036030066,"d":"1.53"},{"v":0.6899100864999999,"d":"0.69"}]
["13215","Muscogee","GA",{"v":0.149515114,"d":"0.15"},{"v":1.0863868174847804,"d":"1.09"},{"v":1.0863868174847804,"d":"1.09"},{"v":0.5170426739999999,"d":"0.52"}]
["13217","Newton","GA",{"v":0.201446959,"d":"0.20"},{"v":1.2935326633356934,"d":"1.29"},{"v":1.2935326633356934,"d":"1.29"},{"v":0.5847063975000001,"d":"0.58"}]
["13219","Oconee","GA",{"v":0.21952227800000002,"d":"0.22"},{"v":1.38428563253165,"d":"1.38"},{"v":1.38428563253165,"d":"1.38"},{"v":0.6356286640000001,"d":"0.64"}]
["13221","Oglethorpe","GA",{"v":0.250877608,"d":"0.25"},{"v":1.494682497940371,"d":"1.49"},{"v":1.4946824979403712,"d":"1.49"},{"v":0.7220738044999999,"d":"0.72"}]
["13223","Paulding","GA",{"v":0.181573204,"d":"0.18"},{"v":1.3069845637484725,"d":"1.31"},{"v":1.3069845637484725,"d":"1.31"},{"v":0.612891043,"d":"0.61"}]
["13225","Peach","GA",{"v":0.218221209,"d":"0.22"},{"v":1.3481322806417324,"d":"1.35"},{"v":1.3481322806417326,"d":"1.35"},{"v":0.5822678825,"d":"0.58"}]
["13227","Pickens","GA",{"v":0.225445267,"d":"0.23"},{"v":1.4666058078378768,"d":"1.47"},{"v":1.4666058078378768,"d":"1.47"},{"v":0.7351180725,"d":"0.74"}]
["13229","Pierce","GA",{"v":0.254282917,"d":"0.25"},{"v":1.3900900299894576,"d":"1.39"},{"v":1.3900900299894579,"d":"1.39"},{"v":0.6250134335,"d":"0.63"}]
["13231","Pike","GA",{"v":0.260351988,"d":"0.26"},{"v":1.4301742912875628,"d":"1.43"},{"v":1.4301742912875628,"d":"1.43"},{"v":0.672594915,"d":"0.67"}]
["13233","Polk","GA",{"v":0.22140023000000003,"d":"0.22"},{"v":1.403804454900957,"d":"1.40"},{"v":1.403804454900957,"d":"1.40"},{"v":0.6491448129999999,"d":"0.65"}]
["13235","Pulaski","GA",{"v":0.245264498,"d":"0.25"},{"v":1.3917600023318242,"d":"1.39"},{"v":1.3917600023318242,"d":"1.39"},{"v":0.5946143595,"d":"0.59"}]
["13237","Putnam","GA",{"v":0.24304483499999996,"d":"0.24"},{"v":1.447701757406123,"d":"1.45"},{"v":1.447701757406123,"d":"1.45"},{"v":0.6801363895,"d":"0.68"}]
["13239","Quitman","GA",{"v":0.242764077,"d":"0.24"},{"v":1.5023621295191352,"d":"1.50"},{"v":1.5023621295191352,"d":"1.50"},{"v":0.6388257345,"d":"0.64"}]
["13241","Rabun","GA",{"v":0.230489975,"d":"0.23"},{"v":1.4797523807179276,"d":"1.48"},{"v":1.4797523807179276,"d":"1.48"},{"v":0.8077318990000001,"d":"0.81"}]
["13243","Randolph","GA",{"v":0.23885117199999997,"d":"0.24"},{"v":1.3550202766494805,"d":"1.36"},{"v":1.3550202766494805,"d":"1.36"},{"v":0.6176804245,"d":"0.62"}]
["13245","Richmond","GA",{"v":0.177056224,"d":"0.18"},{"v":1.2241708260785507,"d":"1.22"},{"v":1.2241708260785507,"d":"1.22"},{"v":0.5147280435,"d":"0.51"}]
["13247","Rockdale","GA",{"v":0.17565466399999996,"d":"0.18"},{"v":1.1814610538147698,"d":"1.18"},{"v":1.1814610538147698,"d":"1.18"},{"v":0.5434532695000001,"d":"0.54"}]
["13249","Schley","GA",{"v":0.256151664,"d":"0.26"},{"v":1.463804756850266,"d":"1.46"},{"v":1.4638047568502661,"d":"1.46"},{"v":0.6832859879999998,"d":"0.68"}]
["13251","Screven","GA",{"v":0.251869057,"d":"0.25"},{"v":1.4064492546618361,"d":"1.41"},{"v":1.4064492546618363,"d":"1.41"},{"v":0.651709322,"d":"0.65"}]
["13253","Seminole","GA",{"v":0.262999142,"d":"0.26"},{"v":1.3751117039321663,"d":"1.38"},{"v":1.3751117039321665,"d":"1.38"},{"v":0.5478234259999999,"d":"0.55"}]
["13255","Spalding","GA",{"v":0.20906254600000002,"d":"0.21"},{"v":1.295880570578124,"d":"1.30"},{"v":1.295880570578124,"d":"1.30"},{"v":0.6016150164999999,"d":"0.60"}]
["13257","Stephens","GA",{"v":0.22565782700000003,"d":"0.23"},{"v":1.4446117188509524,"d":"1.44"},{"v":1.4446117188509526,"d":"1.44"},{"v":0.6647653175,"d":"0.66"}]
["13259","Stewart","GA",{"v":0.259268857,"d":"0.26"},{"v":1.3853350239698845,"d":"1.39"},{"v":1.3853350239698843,"d":"1.39"},{"v":0.707394253,"d":"0.71"}]
["13261","Sumter","GA",{"v":0.232204797,"d":"0.23"},{"v":1.3235811549244165,"d":"1.32"},{"v":1.3235811549244167,"d":"1.32"},{"v":0.5727305795000001,"d":"0.57"}]
["13263","Talbot","GA",{"v":0.24870899900000004,"d":"0.25"},{"v":1.4809450882841304,"d":"1.48"},{"v":1.48094508828413,"d":"1.48"},{"v":0.7270259530000001,"d":"0.73"}]
["13265","Taliaferro","GA",{"v":0.249680925,"d":"0.25"},{"v":1.4366293710586364,"d":"1.44"},{"v":1.4366293710586362,"d":"1.44"},{"v":0.7459485140000001,"d":"0.75"}]
["13267","Tattnall","GA",{"v":0.248849571,"d":"0.25"},{"v":1.3763508276809644,"d":"1.38"},{"v":1.3763508276809644,"d":"1.38"},{"v":0.6190858175000001,"d":"0.62"}]
["13269","Taylor","GA",{"v":0.260848677,"d":"0.26"},{"v":1.4453461340909215,"d":"1.45"},{"v":1.4453461340909215,"d":"1.45"},{"v":0.6586194065000001,"d":"0.66"}]
["13271","Telfair","GA",{"v":0.23396728600000002,"d":"0.23"},{"v":1.3758325883570244,"d":"1.38"},{"v":1.3758325883570244,"d":"1.38"},{"v":0.6437295955,"d":"0.64"}]
["13273","Terrell","GA",{"v":0.244055044,"d":"0.24"},{"v":1.3414256603759676,"d":"1.34"},{"v":1.3414256603759676,"d":"1.34"},{"v":0.585794714,"d":"0.59"}]
["13275","Thomas","GA",{"v":0.233792918,"d":"0.23"},{"v":1.3652956839186703,"d":"1.37"},{"v":1.36529568391867,"d":"1.37"},{"v":0.5815463115,"d":"0.58"}]
["13277","Tift","GA",{"v":0.23117168400000002,"d":"0.23"},{"v":1.3472882894626812,"d":"1.35"},{"v":1.3472882894626812,"d":"1.35"},{"v":0.5446520185,"d":"0.54"}]
["13279","Toombs","GA",{"v":0.23467870500000002,"d":"0.23"},{"v":1.3304304365377455,"d":"1.33"},{"v":1.3304304365377453,"d":"1.33"},{"v":0.5911052715,"d":"0.59"}]
["13281","Towns","GA",{"v":0.24210712200000004,"d":"0.24"},{"v":1.5157239602087798,"d":"1.52"},{"v":1.5157239602087798,"d":"1.52"},{"v":0.799106743,"d":"0.80"}]
["13283","Treutlen","GA",{"v":0.23510911200000004,"d":"0.24"},{"v":1.4367654080339451,"d":"1.44"},{"v":1.436765408033945,"d":"1.44"},{"v":0.6489843940000001,"d":"0.65"}]
["13285","Troup","GA",{"v":0.21437950600000003,"d":"0.21"},{"v":1.3601443213704454,"d":"1.36"},{"v":1.3601443213704454,"d":"1.36"},{"v":0.631149289,"d":"0.63"}]
["13287","Turner","GA",{"v":0.24153263100000003,"d":"0.24"},{"v":1.3477897818186895,"d":"1.35"},{"v":1.3477897818186895,"d":"1.35"},{"v":0.5703782715,"d":"0.57"}]
["13289","Twiggs","GA",{"v":0.253965231,"d":"0.25"},{"v":1.452834011077832,"d":"1.45"},{"v":1.452834011077832,"d":"1.45"},{"v":0.7139718015,"d":"0.71"}]
["13291","Union","GA",{"v":0.242419512,"d":"0.24"},{"v":1.5148963094614667,"d":"1.51"},{"v":1.5148963094614665,"d":"1.51"},{"v":0.78827295,"d":"0.79"}]
["13293","Upson","GA",{"v":0.220991023,"d":"0.22"},{"v":1.3540052571849044,"d":"1.35"},{"v":1.3540052571849044,"d":"1.35"},{"v":0.666615149,"d":"0.67"}]
["13295","Walker","GA",{"v":0.21127969899999996,"d":"0.21"},{"v":1.447387544228271,"d":"1.45"},{"v":1.4473875442282713,"d":"1.45"},{"v":0.655417061,"d":"0.66"}]
["13297","Walton","GA",{"v":0.21214537399999997,"d":"0.21"},{"v":1.396278299906601,"d":"1.40"},{"v":1.396278299906601,"d":"1.40"},{"v":0.604922801,"d":"0.60"}]
["13299","Ware","GA",{"v":0.21913173099999997,"d":"0.22"},{"v":1.3350833976629173,"d":"1.34"},{"v":1.3350833976629175,"d":"1.34"},{"v":0.6144070739999999,"d":"0.61"}]
["13301","Warren","GA",{"v":0.25322260799999996,"d":"0.25"},{"v":1.415279171594317,"d":"1.42"},{"v":1.415279171594317,"d":"1.42"},{"v":0.7079056585,"d":"0.71"}]
["13303","Washington","GA",{"v":0.23175834999999997,"d":"0.23"},{"v":1.3826800934918881,"d":"1.38"},{"v":1.3826800934918881,"d":"1.38"},{"v":0.6690709629999999,"d":"0.67"}]
["13305","Wayne","GA",{"v":0.23569685600000004,"d":"0.24"},{"v":1.378666896146264,"d":"1.38"},{"v":1.378666896146264,"d":"1.38"},{"v":0.6495619335,"d":"0.65"}]
["13307","Webster","GA",{"v":0.265484277,"d":"0.27"},{"v":1.4496404522954254,"d":"1.45"},{"v":1.4496404522954252,"d":"1.45"},{"v":0.6565073525,"d":"0.66"}]
["13309","Wheeler","GA",{"v":0.259239747,"d":"0.26"},{"v":1.4631995488551321,"d":"1.46"},{"v":1.463199548855132,"d":"1.46"},{"v":0.6856287254999999,"d":"0.69"}]
["13311","White","GA",{"v":0.231187952,"d":"0.23"},{"v":1.5143069333621475,"d":"1.51"},{"v":1.5143069333621477,"d":"1.51"},{"v":0.7364882205000001,"d":"0.74"}]
["13313","Whitfield","GA",{"v":0.19472731,"d":"0.19"},{"v":1.438267818037268,"d":"1.44"},{"v":1.438267818037268,"d":"1.44"},{"v":0.597978281,"d":"0.60"}]
["13315","Wilcox","GA",{"v":0.269738277,"d":"0.27"},{"v":1.404282429250787,"d":"1.40"},{"v":1.4042824292507867,"d":"1.40"},{"v":0.641006151,"d":"0.64"}]
["13317","Wilkes","GA",{"v":0.233593298,"d":"0.23"},{"v":1.3973945359043785,"d":"1.40"},{"v":1.3973945359043785,"d":"1.40"},{"v":0.7017400304999999,"d":"0.70"}]
["13319","Wilkinson","GA",{"v":0.255476779,"d":"0.26"},{"v":1.4267485933254678,"d":"1.43"},{"v":1.4267485933254678,"d":"1.43"},{"v":0.7242984240000001,"d":"0.72"}]
["13321","Worth","GA",{"v":0.251841239,"d":"0.25"},{"v":1.3862332154077883,"d":"1.39"},{"v":1.3862332154077883,"d":"1.39"},{"v":0.5955665615000001,"d":"0.60"}]
["15001","Hawaii","HI",{"v":0.12846398800000003,"d":"0.13"},{"v":0.6107324294251778,"d":"0.61"},{"v":0.6107324294251779,"d":"0.61"},{"v":0.24667955399999997,"d":"0.25"}]
["15003","Honolulu","HI",{"v":0.066818175,"d":"0.07"},{"v":0.28042936063477497,"d":"0.28"},{"v":0.28042936063477497,"d":"0.28"},{"v":0.19343471850000002,"d":"0.19"}]
["15005","Kalawao","HI",{"v":0.15238104399999997,"d":"0.15"},{"v":0.6105806616516819,"d":"0.61"},{"v":0.6105806616516819,"d":"0.61"},{"v":0.26974622499999995,"d":"0.27"}]
["15007","Kauai","HI",{"v":0.11706059600000002,"d":"0.12"},{"v":0.6028858370273804,"d":"0.60"},{"v":0.6028858370273804,"d":"0.60"},{"v":0.23099982949999998,"d":"0.23"}]
["15009","Maui","HI",{"v":0.113738535,"d":"0.11"},{"v":0.6063916719195795,"d":"0.61"},{"v":0.6063916719195795,"d":"0.61"},{"v":0.23093105999999997,"d":"0.23"}]
["16001","Ada","ID",{"v":0.276508041,"d":"0.28"},{"v":1.9888388404590032,"d":"1.99"},{"v":1.9888388404590034,"d":"1.99"},{"v":0.5817643085,"d":"0.58"}]
["16003","Adams","ID",{"v":0.35299425100000004,"d":"0.35"},{"v":2.608746706799259,"d":"2.61"},{"v":2.608746706799259,"d":"2.61"},{"v":0.9292875184999999,"d":"0.93"}]
["16005","Bannock","ID",{"v":0.292460494,"d":"0.29"},{"v":2.322900456499321,"d":"2.32"},{"v":2.3229004564993216,"d":"2.32"},{"v":0.7093631385,"d":"0.71"}]
["16007","Bear Lake","ID",{"v":0.365457023,"d":"0.37"},{"v":2.4474061373744664,"d":"2.45"},{"v":2.4474061373744664,"d":"2.45"},{"v":0.856654793,"d":"0.86"}]
["16009","Benewah","ID",{"v":0.31918855299999993,"d":"0.32"},{"v":2.5516469552867425,"d":"2.55"},{"v":2.5516469552867425,"d":"2.55"},{"v":0.9258934120000001,"d":"0.93"}]
["16011","Bingham","ID",{"v":0.340010955,"d":"0.34"},{"v":2.3739227527642695,"d":"2.37"},{"v":2.3739227527642695,"d":"2.37"},{"v":0.7536800774999999,"d":"0.75"}]
["16013","Blaine","ID",{"v":0.314618512,"d":"0.31"},{"v":2.1281066929872705,"d":"2.13"},{"v":2.128106692987271,"d":"2.13"},{"v":0.7234111210000002,"d":"0.72"}]
["16015","Boise","ID",{"v":0.351183209,"d":"0.35"},{"v":2.6015111722781366,"d":"2.60"},{"v":2.6015111722781366,"d":"2.60"},{"v":0.9273365459999999,"d":"0.93"}]
["16017","Bonner","ID",{"v":0.309236268,"d":"0.31"},{"v":2.545996762618174,"d":"2.55"},{"v":2.5459967626181745,"d":"2.55"},{"v":0.9924610765000001,"d":"0.99"}]
["16019","Bonneville","ID",{"v":0.29444139499999994,"d":"0.29"},{"v":2.382392472642729,"d":"2.38"},{"v":2.382392472642729,"d":"2.38"},{"v":0.7148174334999999,"d":"0.71"}]
["16021","Boundary","ID",{"v":0.3087489319999999,"d":"0.31"},{"v":2.535881368308147,"d":"2.54"},{"v":2.5358813683081474,"d":"2.54"},{"v":1.031130648,"d":"1.03"}]
["16023","Butte","ID",{"v":0.379200256,"d":"0.38"},{"v":2.442832378563426,"d":"2.44"},{"v":2.442832378563426,"d":"2.44"},{"v":0.8125070655000001,"d":"0.81"}]
["16025","Camas","ID",{"v":0.363478519,"d":"0.36"},{"v":2.5575926537468394,"d":"2.56"},{"v":2.5575926537468394,"d":"2.56"},{"v":0.8678382550000002,"d":"0.87"}]
["16027","Canyon","ID",{"v":0.295172222,"d":"0.30"},{"v":2.0595827093427497,"d":"2.06"},{"v":2.0595827093427497,"d":"2.06"},{"v":0.622165713,"d":"0.62"}]
["16029","Caribou","ID",{"v":0.328657519,"d":"0.33"},{"v":2.3842793485616185,"d":"2.38"},{"v":2.384279348561619,"d":"2.38"},{"v":0.8132196084999999,"d":"0.81"}]
["16031","Cassia","ID",{"v":0.326578579,"d":"0.33"},{"v":2.432761210774432,"d":"2.43"},{"v":2.4327612107744323,"d":"2.43"},{"v":0.7583385945,"d":"0.76"}]
["16033","Clark","ID",{"v":0.365630955,"d":"0.37"},{"v":2.485817460863414,"d":"2.49"},{"v":2.485817460863414,"d":"2.49"},{"v":0.8367706810000001,"d":"0.84"}]
["16035","Clearwater","ID",{"v":0.291695358,"d":"0.29"},{"v":2.709116725371388,"d":"2.71"},{"v":2.709116725371388,"d":"2.71"},{"v":1.0293561225,"d":"1.03"}]
["16037","Custer","ID",{"v":0.35993853500000006,"d":"0.36"},{"v":2.566696275022518,"d":"2.57"},{"v":2.566696275022518,"d":"2.57"},{"v":0.8753282365,"d":"0.88"}]
["16039","Elmore","ID",{"v":0.309806682,"d":"0.31"},{"v":2.4236207432421906,"d":"2.42"},{"v":2.423620743242191,"d":"2.42"},{"v":0.7468042850000001,"d":"0.75"}]
["16041","Franklin","ID",{"v":0.33567287500000004,"d":"0.34"},{"v":2.4381425404731685,"d":"2.44"},{"v":2.4381425404731685,"d":"2.44"},{"v":0.8149362110000001,"d":"0.81"}]
["16043","Fremont","ID",{"v":0.34022962399999995,"d":"0.34"},{"v":2.4471881569774903,"d":"2.45"},{"v":2.4471881569774903,"d":"2.45"},{"v":0.8473263560000001,"d":"0.85"}]
["16045","Gem","ID",{"v":0.335335259,"d":"0.34"},{"v":2.1904718312087454,"d":"2.19"},{"v":2.190471831208745,"d":"2.19"},{"v":0.7137196074999999,"d":"0.71"}]
["16047","Gooding","ID",{"v":0.346467272,"d":"0.35"},{"v":2.2956071487094207,"d":"2.30"},{"v":2.2956071487094207,"d":"2.30"},{"v":0.7204691350000001,"d":"0.72"}]
["16049","Idaho","ID",{"v":0.3176347299999999,"d":"0.32"},{"v":2.674750470845539,"d":"2.67"},{"v":2.674750470845539,"d":"2.67"},{"v":0.994701283,"d":"0.99"}]
["16051","Jefferson","ID",{"v":0.353770325,"d":"0.35"},{"v":2.37935469228872,"d":"2.38"},{"v":2.37935469228872,"d":"2.38"},{"v":0.7590828379999999,"d":"0.76"}]
["16053","Jerome","ID",{"v":0.34725735099999994,"d":"0.35"},{"v":2.2776052311044563,"d":"2.28"},{"v":2.277605231104457,"d":"2.28"},{"v":0.7083155245,"d":"0.71"}]
["16055","Kootenai","ID",{"v":0.26841016,"d":"0.27"},{"v":2.3803026770285904,"d":"2.38"},{"v":2.380302677028591,"d":"2.38"},{"v":0.8599854825000001,"d":"0.86"}]
["16057","Latah","ID",{"v":0.29511586,"d":"0.30"},{"v":2.26024404468735,"d":"2.26"},{"v":2.26024404468735,"d":"2.26"},{"v":0.7953150925000001,"d":"0.80"}]
["16059","Lemhi","ID",{"v":0.314243543,"d":"0.31"},{"v":2.605848518111387,"d":"2.61"},{"v":2.6058485181113866,"d":"2.61"},{"v":0.8717987325,"d":"0.87"}]
["16061","Lewis","ID",{"v":0.382962987,"d":"0.38"},{"v":2.3402377793200544,"d":"2.34"},{"v":2.340237779320054,"d":"2.34"},{"v":0.815763152,"d":"0.82"}]
["16063","Lincoln","ID",{"v":0.38821357,"d":"0.39"},{"v":2.3307816052019312,"d":"2.33"},{"v":2.3307816052019312,"d":"2.33"},{"v":0.7764591175000001,"d":"0.78"}]
["16065","Madison","ID",{"v":0.27321362500000007,"d":"0.27"},{"v":2.3460473305187217,"d":"2.35"},{"v":2.3460473305187217,"d":"2.35"},{"v":0.725754604,"d":"0.73"}]
["16067","Minidoka","ID",{"v":0.33946468,"d":"0.34"},{"v":2.2732410565028047,"d":"2.27"},{"v":2.2732410565028043,"d":"2.27"},{"v":0.6981092210000001,"d":"0.70"}]
["16069","Nez Perce","ID",{"v":0.30516135600000005,"d":"0.31"},{"v":2.2717398289773802,"d":"2.27"},{"v":2.2717398289773802,"d":"2.27"},{"v":0.691335294,"d":"0.69"}]
["16071","Oneida","ID",{"v":0.374890344,"d":"0.37"},{"v":2.469275992209577,"d":"2.47"},{"v":2.4692759922095773,"d":"2.47"},{"v":0.8252501550000001,"d":"0.83"}]
["16073","Owyhee","ID",{"v":0.369275072,"d":"0.37"},{"v":2.370182623532528,"d":"2.37"},{"v":2.370182623532528,"d":"2.37"},{"v":0.7645757189999999,"d":"0.76"}]
["16075","Payette","ID",{"v":0.347053145,"d":"0.35"},{"v":2.1632115968607906,"d":"2.16"},{"v":2.1632115968607906,"d":"2.16"},{"v":0.6765747785,"d":"0.68"}]
["16077","Power","ID",{"v":0.32847314699999997,"d":"0.33"},{"v":2.378947032282694,"d":"2.38"},{"v":2.378947032282694,"d":"2.38"},{"v":0.7458755105,"d":"0.75"}]
["16079","Shoshone","ID",{"v":0.283842258,"d":"0.28"},{"v":2.5704299359718514,"d":"2.57"},{"v":2.570429935971851,"d":"2.57"},{"v":1.0506851435,"d":"1.05"}]
["16081","Teton","ID",{"v":0.359568794,"d":"0.36"},{"v":2.5110726948598785,"d":"2.51"},{"v":2.5110726948598785,"d":"2.51"},{"v":0.8940538454999999,"d":"0.89"}]
["16083","Twin Falls","ID",{"v":0.32217074399999995,"d":"0.32"},{"v":2.2522492931170097,"d":"2.25"},{"v":2.2522492931170097,"d":"2.25"},{"v":0.6782064915,"d":"0.68"}]
["16085","Valley","ID",{"v":0.350536279,"d":"0.35"},{"v":2.5768929857375524,"d":"2.58"},{"v":2.5768929857375524,"d":"2.58"},{"v":0.9143178805000001,"d":"0.91"}]
["16087","Washington","ID",{"v":0.34232074900000004,"d":"0.34"},{"v":2.1660786616022154,"d":"2.17"},{"v":2.1660786616022154,"d":"2.17"},{"v":0.7097437404999999,"d":"0.71"}]
["17001","Adams","IL",{"v":0.316821132,"d":"0.32"},{"v":2.1439871855796264,"d":"2.14"},{"v":2.1439871855796264,"d":"2.14"},{"v":0.7413805349999999,"d":"0.74"}]
["17003","Alexander","IL",{"v":0.325319816,"d":"0.33"},{"v":2.135543859346215,"d":"2.14"},{"v":2.135543859346215,"d":"2.14"},{"v":0.8495074310000001,"d":"0.85"}]
["17005","Bond","IL",{"v":0.35149455099999993,"d":"0.35"},{"v":2.194440590589933,"d":"2.19"},{"v":2.194440590589933,"d":"2.19"},{"v":0.7810406334999999,"d":"0.78"}]
["17007","Boone","IL",{"v":0.30127081799999994,"d":"0.30"},{"v":2.157144834262073,"d":"2.16"},{"v":2.157144834262073,"d":"2.16"},{"v":0.676505293,"d":"0.68"}]
["17009","Brown","IL",{"v":0.329294267,"d":"0.33"},{"v":2.26269722054379,"d":"2.26"},{"v":2.2626972205437905,"d":"2.26"},{"v":0.8434377515000001,"d":"0.84"}]
["17011","Bureau","IL",{"v":0.34192832,"d":"0.34"},{"v":2.2177684307467347,"d":"2.22"},{"v":2.2177684307467347,"d":"2.22"},{"v":0.7562600685,"d":"0.76"}]
["17013","Calhoun","IL",{"v":0.37799532099999994,"d":"0.38"},{"v":2.250484132052694,"d":"2.25"},{"v":2.250484132052694,"d":"2.25"},{"v":0.879955958,"d":"0.88"}]
["17015","Carroll","IL",{"v":0.361076468,"d":"0.36"},{"v":2.265880275986188,"d":"2.27"},{"v":2.265880275986188,"d":"2.27"},{"v":0.8075735010000001,"d":"0.81"}]
["17017","Cass","IL",{"v":0.34358038600000007,"d":"0.34"},{"v":2.1204760710630195,"d":"2.12"},{"v":2.1204760710630195,"d":"2.12"},{"v":0.7700988784999999,"d":"0.77"}]
["17019","Champaign","IL",{"v":0.28153137699999997,"d":"0.28"},{"v":2.1380970213139037,"d":"2.14"},{"v":2.1380970213139032,"d":"2.14"},{"v":0.6313657455,"d":"0.63"}]
["17021","Christian","IL",{"v":0.34215785,"d":"0.34"},{"v":2.061922110403965,"d":"2.06"},{"v":2.061922110403965,"d":"2.06"},{"v":0.7039646595,"d":"0.70"}]
["17023","Clark","IL",{"v":0.346831818,"d":"0.35"},{"v":2.159932536040173,"d":"2.16"},{"v":2.159932536040173,"d":"2.16"},{"v":0.7742899215000002,"d":"0.77"}]
["17025","Clay","IL",{"v":0.3536646480000001,"d":"0.35"},{"v":2.181663212639885,"d":"2.18"},{"v":2.1816632126398856,"d":"2.18"},{"v":0.7759196885,"d":"0.78"}]
["17027","Clinton","IL",{"v":0.3385851730000001,"d":"0.34"},{"v":2.0533995363964404,"d":"2.05"},{"v":2.05339953639644,"d":"2.05"},{"v":0.7154534470000001,"d":"0.72"}]
["17029","Coles","IL",{"v":0.312483798,"d":"0.31"},{"v":2.0735679798500275,"d":"2.07"},{"v":2.0735679798500275,"d":"2.07"},{"v":0.679712919,"d":"0.68"}]
["17031","Cook","IL",{"v":0.047058864,"d":"0.05"},{"v":2.8719727846521824E-7,"d":"0.00"},{"v":2.8719727846521824E-7,"d":"0.00"},{"v":0.40491439700000004,"d":"0.40"}]
["17033","Crawford","IL",{"v":0.352170184,"d":"0.35"},{"v":2.1256585766460745,"d":"2.13"},{"v":2.1256585766460745,"d":"2.13"},{"v":0.7720273499999998,"d":"0.77"}]
["17035","Cumberland","IL",{"v":0.39214992600000004,"d":"0.39"},{"v":2.204985241774117,"d":"2.20"},{"v":2.2049852417741174,"d":"2.20"},{"v":0.8097795624999998,"d":"0.81"}]
["17037","De Kalb","IL",{"v":0.30604405,"d":"0.31"},{"v":2.186319307675252,"d":"2.19"},{"v":2.186319307675252,"d":"2.19"},{"v":0.6645898705,"d":"0.66"}]
["17039","Dewitt","IL",{"v":0.34355166800000003,"d":"0.34"},{"v":2.11516052175285,"d":"2.12"},{"v":2.11516052175285,"d":"2.12"},{"v":0.724727327,"d":"0.72"}]
["17041","Douglas","IL",{"v":0.365245413,"d":"0.37"},{"v":2.0970026338851433,"d":"2.10"},{"v":2.0970026338851433,"d":"2.10"},{"v":0.714406301,"d":"0.71"}]
["17043","Du Page","IL",{"v":0.11802202799999999,"d":"0.12"},{"v":0.009534567578390917,"d":"0.01"},{"v":0.00953456757839092,"d":"0.01"},{"v":0.5142430875,"d":"0.51"}]
["17045","Edgar","IL",{"v":0.35073578999999994,"d":"0.35"},{"v":2.106788295190006,"d":"2.11"},{"v":2.1067882951900057,"d":"2.11"},{"v":0.7215035224999999,"d":"0.72"}]
["17047","Edwards","IL",{"v":0.3943779439999999,"d":"0.39"},{"v":2.0882815669282753,"d":"2.09"},{"v":2.0882815669282757,"d":"2.09"},{"v":0.7888817764999999,"d":"0.79"}]
["17049","Effingham","IL",{"v":0.339508419,"d":"0.34"},{"v":2.142199191856279,"d":"2.14"},{"v":2.1421991918562786,"d":"2.14"},{"v":0.7703170605,"d":"0.77"}]
["17051","Fayette","IL",{"v":0.356956234,"d":"0.36"},{"v":2.177985004509409,"d":"2.18"},{"v":2.177985004509409,"d":"2.18"},{"v":0.797974848,"d":"0.80"}]
["17053","Ford","IL",{"v":0.340899774,"d":"0.34"},{"v":2.1581479668303625,"d":"2.16"},{"v":2.158147966830363,"d":"2.16"},{"v":0.6957538809999999,"d":"0.70"}]
["17055","Franklin","IL",{"v":0.33249781500000003,"d":"0.33"},{"v":2.077788916942984,"d":"2.08"},{"v":2.077788916942984,"d":"2.08"},{"v":0.7493396979999999,"d":"0.75"}]
["17057","Fulton","IL",{"v":0.33941120399999997,"d":"0.34"},{"v":2.175742832411521,"d":"2.18"},{"v":2.1757428324115216,"d":"2.18"},{"v":0.8190725915,"d":"0.82"}]
["17059","Gallatin","IL",{"v":0.39410140900000007,"d":"0.39"},{"v":2.0519313698827513,"d":"2.05"},{"v":2.0519313698827513,"d":"2.05"},{"v":0.8273484839999998,"d":"0.83"}]
["17061","Greene","IL",{"v":0.3563582350000001,"d":"0.36"},{"v":2.110507571047791,"d":"2.11"},{"v":2.110507571047791,"d":"2.11"},{"v":0.805744234,"d":"0.81"}]
["17063","Grundy","IL",{"v":0.319501996,"d":"0.32"},{"v":2.1986008637565315,"d":"2.20"},{"v":2.1986008637565315,"d":"2.20"},{"v":0.6907105025,"d":"0.69"}]
["17065","Hamilton","IL",{"v":0.36283959899999996,"d":"0.36"},{"v":2.108895906676105,"d":"2.11"},{"v":2.108895906676105,"d":"2.11"},{"v":0.7622387684999999,"d":"0.76"}]
["17067","Hancock","IL",{"v":0.360985554,"d":"0.36"},{"v":2.196056166034968,"d":"2.20"},{"v":2.1960561660349684,"d":"2.20"},{"v":0.7864967445000001,"d":"0.79"}]
["17069","Hardin","IL",{"v":0.356234632,"d":"0.36"},{"v":2.1692503096840214,"d":"2.17"},{"v":2.169250309684021,"d":"2.17"},{"v":1.0094334790000001,"d":"1.01"}]
["17071","Henderson","IL",{"v":0.389825598,"d":"0.39"},{"v":2.1913761045738434,"d":"2.19"},{"v":2.191376104573844,"d":"2.19"},{"v":0.8164885765,"d":"0.82"}]
["17073","Henry","IL",{"v":0.334500393,"d":"0.33"},{"v":2.20015478165709,"d":"2.20"},{"v":2.2001547816570906,"d":"2.20"},{"v":0.7405361205,"d":"0.74"}]
["17075","Iroquois","IL",{"v":0.37064018399999993,"d":"0.37"},{"v":2.1713619869561556,"d":"2.17"},{"v":2.171361986956156,"d":"2.17"},{"v":0.7466639559999999,"d":"0.75"}]
["17077","Jackson","IL",{"v":0.296000713,"d":"0.30"},{"v":2.084403535697418,"d":"2.08"},{"v":2.0844035356974184,"d":"2.08"},{"v":0.8131923574999999,"d":"0.81"}]
["17079","Jasper","IL",{"v":0.361758978,"d":"0.36"},{"v":2.18591903853967,"d":"2.19"},{"v":2.1859190385396694,"d":"2.19"},{"v":0.765982305,"d":"0.77"}]
["17081","Jefferson","IL",{"v":0.33603729600000004,"d":"0.34"},{"v":2.143803622501966,"d":"2.14"},{"v":2.143803622501966,"d":"2.14"},{"v":0.759011294,"d":"0.76"}]
["17083","Jersey","IL",{"v":0.335015004,"d":"0.34"},{"v":2.1896323556955357,"d":"2.19"},{"v":2.1896323556955357,"d":"2.19"},{"v":0.8147672730000001,"d":"0.81"}]
["17085","Jo Daviess","IL",{"v":0.354165739,"d":"0.35"},{"v":2.295464103161681,"d":"2.30"},{"v":2.295464103161681,"d":"2.30"},{"v":0.8164211015,"d":"0.82"}]
["17087","Johnson","IL",{"v":0.362376181,"d":"0.36"},{"v":2.2392716068484275,"d":"2.24"},{"v":2.2392716068484275,"d":"2.24"},{"v":0.9498092210000001,"d":"0.95"}]
["17089","Kane","IL",{"v":0.22640759900000001,"d":"0.23"},{"v":1.7830186479125731,"d":"1.78"},{"v":1.7830186479125731,"d":"1.78"},{"v":0.5937102905,"d":"0.59"}]
["17091","Kankakee","IL",{"v":0.311882318,"d":"0.31"},{"v":2.0907355596311996,"d":"2.09"},{"v":2.0907355596311996,"d":"2.09"},{"v":0.672271263,"d":"0.67"}]
["17093","Kendall","IL",{"v":0.29046555699999993,"d":"0.29"},{"v":2.1492679295947363,"d":"2.15"},{"v":2.1492679295947354,"d":"2.15"},{"v":0.6351283519999998,"d":"0.64"}]
["17095","Knox","IL",{"v":0.308181139,"d":"0.31"},{"v":2.1304979385255574,"d":"2.13"},{"v":2.1304979385255574,"d":"2.13"},{"v":0.7138418940000001,"d":"0.71"}]
["17097","Lake","IL",{"v":0.180632962,"d":"0.18"},{"v":0.8044491306189429,"d":"0.80"},{"v":0.8044491306189429,"d":"0.80"},{"v":0.5809077485,"d":"0.58"}]
["17099","La Salle","IL",{"v":0.315359272,"d":"0.32"},{"v":2.1505256842289744,"d":"2.15"},{"v":2.150525684228975,"d":"2.15"},{"v":0.700167167,"d":"0.70"}]
["17101","Lawrence","IL",{"v":0.33827242,"d":"0.34"},{"v":2.1031429360199922,"d":"2.10"},{"v":2.1031429360199922,"d":"2.10"},{"v":0.747074355,"d":"0.75"}]
["17103","Lee","IL",{"v":0.34048923099999995,"d":"0.34"},{"v":2.2036472122628497,"d":"2.20"},{"v":2.2036472122628497,"d":"2.20"},{"v":0.7502214955,"d":"0.75"}]
["17105","Livingston","IL",{"v":0.342147409,"d":"0.34"},{"v":2.1453653259737533,"d":"2.15"},{"v":2.1453653259737533,"d":"2.15"},{"v":0.7021958275000001,"d":"0.70"}]
["17107","Logan","IL",{"v":0.340485433,"d":"0.34"},{"v":2.1247537921724753,"d":"2.12"},{"v":2.1247537921724757,"d":"2.12"},{"v":0.7081677409999999,"d":"0.71"}]
["17109","McDonough","IL",{"v":0.31603354399999994,"d":"0.32"},{"v":2.179570701842761,"d":"2.18"},{"v":2.1795707018427604,"d":"2.18"},{"v":0.7192682410000001,"d":"0.72"}]
["17111","McHenry","IL",{"v":0.266780717,"d":"0.27"},{"v":2.0878477215980262,"d":"2.09"},{"v":2.0878477215980267,"d":"2.09"},{"v":0.6531152575,"d":"0.65"}]
["17113","Mclean","IL",{"v":0.299044127,"d":"0.30"},{"v":2.1019261856281934,"d":"2.10"},{"v":2.1019261856281934,"d":"2.10"},{"v":0.647924777,"d":"0.65"}]
["17115","Macon","IL",{"v":0.29447696999999995,"d":"0.29"},{"v":2.088027718653729,"d":"2.09"},{"v":2.088027718653729,"d":"2.09"},{"v":0.648839556,"d":"0.65"}]
["17117","Macoupin","IL",{"v":0.342308614,"d":"0.34"},{"v":2.1123653431495204,"d":"2.11"},{"v":2.11236534314952,"d":"2.11"},{"v":0.7740936715000001,"d":"0.77"}]
["17119","Madison","IL",{"v":0.2790385429999999,"d":"0.28"},{"v":2.0230184470441923,"d":"2.02"},{"v":2.0230184470441923,"d":"2.02"},{"v":0.664606294,"d":"0.66"}]
["17121","Marion","IL",{"v":0.325878043,"d":"0.33"},{"v":2.1192698789714055,"d":"2.12"},{"v":2.1192698789714055,"d":"2.12"},{"v":0.7590132669999999,"d":"0.76"}]
["17123","Marshall","IL",{"v":0.39285287099999994,"d":"0.39"},{"v":2.171394277388826,"d":"2.17"},{"v":2.171394277388826,"d":"2.17"},{"v":0.800557146,"d":"0.80"}]
["17125","Mason","IL",{"v":0.36809777800000004,"d":"0.37"},{"v":2.18591878255098,"d":"2.19"},{"v":2.18591878255098,"d":"2.19"},{"v":0.7824935419999998,"d":"0.78"}]
["17127","Massac","IL",{"v":0.327129283,"d":"0.33"},{"v":2.100258658675486,"d":"2.10"},{"v":2.100258658675486,"d":"2.10"},{"v":0.7948838989999999,"d":"0.79"}]
["17129","Menard","IL",{"v":0.364087388,"d":"0.36"},{"v":2.1522364480031277,"d":"2.15"},{"v":2.1522364480031277,"d":"2.15"},{"v":0.7722785035,"d":"0.77"}]
["17131","Mercer","IL",{"v":0.36111574199999996,"d":"0.36"},{"v":2.285772431366755,"d":"2.29"},{"v":2.285772431366755,"d":"2.29"},{"v":0.7922703855000001,"d":"0.79"}]
["17133","Monroe","IL",{"v":0.328397892,"d":"0.33"},{"v":2.0669993830923215,"d":"2.07"},{"v":2.066999383092322,"d":"2.07"},{"v":0.7411627725000001,"d":"0.74"}]
["17135","Montgomery","IL",{"v":0.339794039,"d":"0.34"},{"v":2.1106056864432254,"d":"2.11"},{"v":2.1106056864432254,"d":"2.11"},{"v":0.7264759139999999,"d":"0.73"}]
["17137","Morgan","IL",{"v":0.329921337,"d":"0.33"},{"v":2.0822558093447308,"d":"2.08"},{"v":2.0822558093447308,"d":"2.08"},{"v":0.7130884339999999,"d":"0.71"}]
["17139","Moultrie","IL",{"v":0.366922566,"d":"0.37"},{"v":2.102062332417844,"d":"2.10"},{"v":2.102062332417844,"d":"2.10"},{"v":0.734391028,"d":"0.73"}]
["17141","Ogle","IL",{"v":0.329130767,"d":"0.33"},{"v":2.2181315667306536,"d":"2.22"},{"v":2.218131566730653,"d":"2.22"},{"v":0.7507074490000001,"d":"0.75"}]
["17143","Peoria","IL",{"v":0.268970173,"d":"0.27"},{"v":2.0865509113149874,"d":"2.09"},{"v":2.086550911314988,"d":"2.09"},{"v":0.7001909865,"d":"0.70"}]
["17145","Perry","IL",{"v":0.33637001799999994,"d":"0.34"},{"v":2.0643926221246156,"d":"2.06"},{"v":2.0643926221246156,"d":"2.06"},{"v":0.7510395400000002,"d":"0.75"}]
["17147","Piatt","IL",{"v":0.3612782950000001,"d":"0.36"},{"v":2.130994327533548,"d":"2.13"},{"v":2.130994327533548,"d":"2.13"},{"v":0.744022852,"d":"0.74"}]
["17149","Pike","IL",{"v":0.356815186,"d":"0.36"},{"v":2.1028272025646992,"d":"2.10"},{"v":2.1028272025646992,"d":"2.10"},{"v":0.8193078755,"d":"0.82"}]
["17151","Pope","IL",{"v":0.35541111499999994,"d":"0.36"},{"v":2.223193979970562,"d":"2.22"},{"v":2.2231939799705622,"d":"2.22"},{"v":1.0008312405,"d":"1.00"}]
["17153","Pulaski","IL",{"v":0.38523334800000003,"d":"0.39"},{"v":2.1145339454394585,"d":"2.11"},{"v":2.114533945439459,"d":"2.11"},{"v":0.8426001865,"d":"0.84"}]
["17155","Putnam","IL",{"v":0.37991218900000007,"d":"0.38"},{"v":2.256435255563281,"d":"2.26"},{"v":2.256435255563281,"d":"2.26"},{"v":0.8417130380000001,"d":"0.84"}]
["17157","Randolph","IL",{"v":0.33774944,"d":"0.34"},{"v":2.083278910385431,"d":"2.08"},{"v":2.083278910385431,"d":"2.08"},{"v":0.754501104,"d":"0.75"}]
["17159","Richland","IL",{"v":0.332983255,"d":"0.33"},{"v":2.1006210635278726,"d":"2.10"},{"v":2.1006210635278726,"d":"2.10"},{"v":0.7313732355,"d":"0.73"}]
["17161","Rock Island","IL",{"v":0.265542369,"d":"0.27"},{"v":2.1236213051986987,"d":"2.12"},{"v":2.123621305198699,"d":"2.12"},{"v":0.6839266945000001,"d":"0.68"}]
["17163","St Clair","IL",{"v":0.275535889,"d":"0.28"},{"v":1.9425492855430835,"d":"1.94"},{"v":1.9425492855430835,"d":"1.94"},{"v":0.6393834165,"d":"0.64"}]
["17165","Saline","IL",{"v":0.325510542,"d":"0.33"},{"v":2.0659504945818075,"d":"2.07"},{"v":2.0659504945818075,"d":"2.07"},{"v":0.7743614975,"d":"0.77"}]
["17167","Sangamon","IL",{"v":0.29736519999999994,"d":"0.30"},{"v":2.0356257905050823,"d":"2.04"},{"v":2.0356257905050823,"d":"2.04"},{"v":0.6421587509999999,"d":"0.64"}]
["17169","Schuyler","IL",{"v":0.3319968649999999,"d":"0.33"},{"v":2.260810458933628,"d":"2.26"},{"v":2.260810458933628,"d":"2.26"},{"v":0.832145444,"d":"0.83"}]
["17171","Scott","IL",{"v":0.389047149,"d":"0.39"},{"v":2.1349981131317333,"d":"2.13"},{"v":2.1349981131317333,"d":"2.13"},{"v":0.8222706670000001,"d":"0.82"}]
["17173","Shelby","IL",{"v":0.37075998300000007,"d":"0.37"},{"v":2.130345836004323,"d":"2.13"},{"v":2.1303458360043224,"d":"2.13"},{"v":0.7729197165,"d":"0.77"}]
["17175","Stark","IL",{"v":0.3995721589999999,"d":"0.40"},{"v":2.179970224136574,"d":"2.18"},{"v":2.179970224136574,"d":"2.18"},{"v":0.7841024875000001,"d":"0.78"}]
["17177","Stephenson","IL",{"v":0.322985075,"d":"0.32"},{"v":2.198959276622378,"d":"2.20"},{"v":2.198959276622378,"d":"2.20"},{"v":0.7245549555,"d":"0.72"}]
["17179","Tazewell","IL",{"v":0.29834180499999996,"d":"0.30"},{"v":2.0970716425127045,"d":"2.10"},{"v":2.097071642512704,"d":"2.10"},{"v":0.6737217455,"d":"0.67"}]
["17181","Union","IL",{"v":0.327663347,"d":"0.33"},{"v":2.183115578993478,"d":"2.18"},{"v":2.183115578993478,"d":"2.18"},{"v":0.9135834869999999,"d":"0.91"}]
["17183","Vermilion","IL",{"v":0.317865665,"d":"0.32"},{"v":2.156905305496384,"d":"2.16"},{"v":2.156905305496384,"d":"2.16"},{"v":0.699610964,"d":"0.70"}]
["17185","Wabash","IL",{"v":0.33207795600000006,"d":"0.33"},{"v":2.062026413080346,"d":"2.06"},{"v":2.0620264130803463,"d":"2.06"},{"v":0.7022708995000001,"d":"0.70"}]
["17187","Warren","IL",{"v":0.342812024,"d":"0.34"},{"v":2.1723087751834873,"d":"2.17"},{"v":2.172308775183487,"d":"2.17"},{"v":0.7282741110000001,"d":"0.73"}]
["17189","Washington","IL",{"v":0.36943363600000007,"d":"0.37"},{"v":2.1221024672226543,"d":"2.12"},{"v":2.1221024672226543,"d":"2.12"},{"v":0.7642994074999999,"d":"0.76"}]
["17191","Wayne","IL",{"v":0.362376079,"d":"0.36"},{"v":2.129669224367069,"d":"2.13"},{"v":2.129669224367069,"d":"2.13"},{"v":0.7523577865000001,"d":"0.75"}]
["17193","White","IL",{"v":0.3598310029999999,"d":"0.36"},{"v":2.043581969887925,"d":"2.04"},{"v":2.043581969887925,"d":"2.04"},{"v":0.7528968114999999,"d":"0.75"}]
["17195","Whiteside","IL",{"v":0.322781289,"d":"0.32"},{"v":2.202356497639572,"d":"2.20"},{"v":2.202356497639572,"d":"2.20"},{"v":0.719172565,"d":"0.72"}]
["17197","Will","IL",{"v":0.243322511,"d":"0.24"},{"v":1.965211981927188,"d":"1.97"},{"v":1.965211981927188,"d":"1.97"},{"v":0.6025887320000001,"d":"0.60"}]
["17199","Williamson","IL",{"v":0.306113919,"d":"0.31"},{"v":2.095738792032312,"d":"2.10"},{"v":2.095738792032312,"d":"2.10"},{"v":0.786690829,"d":"0.79"}]
["17201","Winnebago","IL",{"v":0.25404877299999995,"d":"0.25"},{"v":2.004659170906937,"d":"2.00"},{"v":2.004659170906937,"d":"2.00"},{"v":0.648324561,"d":"0.65"}]
["17203","Woodford","IL",{"v":0.350138311,"d":"0.35"},{"v":2.1462718312210503,"d":"2.15"},{"v":2.14627183122105,"d":"2.15"},{"v":0.7411005835000001,"d":"0.74"}]
["18001","Adams","IN",{"v":0.34140666900000005,"d":"0.34"},{"v":2.301017619479966,"d":"2.30"},{"v":2.301017619479966,"d":"2.30"},{"v":0.7443404330000001,"d":"0.74"}]
["18003","Allen","IN",{"v":0.263685292,"d":"0.26"},{"v":2.1036568588869327,"d":"2.10"},{"v":2.103656858886932,"d":"2.10"},{"v":0.6600820519999999,"d":"0.66"}]
["18005","Bartholomew","IN",{"v":0.313628041,"d":"0.31"},{"v":2.239004757392028,"d":"2.24"},{"v":2.239004757392028,"d":"2.24"},{"v":0.7567023635,"d":"0.76"}]
["18007","Benton","IN",{"v":0.410219952,"d":"0.41"},{"v":2.2901044236892094,"d":"2.29"},{"v":2.290104423689209,"d":"2.29"},{"v":0.8110988915,"d":"0.81"}]
["18009","Blackford","IN",{"v":0.355370864,"d":"0.36"},{"v":2.283090429844979,"d":"2.28"},{"v":2.283090429844979,"d":"2.28"},{"v":0.7567741799999999,"d":"0.76"}]
["18011","Boone","IN",{"v":0.33518053,"d":"0.34"},{"v":2.2227689578034324,"d":"2.22"},{"v":2.2227689578034324,"d":"2.22"},{"v":0.7102081975000001,"d":"0.71"}]
["18013","Brown","IN",{"v":0.36195688600000003,"d":"0.36"},{"v":2.3628825358622776,"d":"2.36"},{"v":2.362882535862278,"d":"2.36"},{"v":1.077914539,"d":"1.08"}]
["18015","Carroll","IN",{"v":0.380345627,"d":"0.38"},{"v":2.322999598639035,"d":"2.32"},{"v":2.3229995986390355,"d":"2.32"},{"v":0.8179343964999998,"d":"0.82"}]
["18017","Cass","IN",{"v":0.341849779,"d":"0.34"},{"v":2.226140143237785,"d":"2.23"},{"v":2.226140143237785,"d":"2.23"},{"v":0.769625591,"d":"0.77"}]
["18019","Clark","IN",{"v":0.288408647,"d":"0.29"},{"v":2.162466718351231,"d":"2.16"},{"v":2.162466718351231,"d":"2.16"},{"v":0.7781189619999999,"d":"0.78"}]
["18021","Clay","IN",{"v":0.347391807,"d":"0.35"},{"v":2.326146243572243,"d":"2.33"},{"v":2.326146243572243,"d":"2.33"},{"v":0.834147691,"d":"0.83"}]
["18023","Clinton","IN",{"v":0.354783021,"d":"0.35"},{"v":2.2091279330944187,"d":"2.21"},{"v":2.2091279330944187,"d":"2.21"},{"v":0.7465498335,"d":"0.75"}]
["18025","Crawford","IN",{"v":0.36682383,"d":"0.37"},{"v":2.3789007285596018,"d":"2.38"},{"v":2.378900728559602,"d":"2.38"},{"v":1.0168037675000001,"d":"1.02"}]
["18027","Daviess","IN",{"v":0.35617234400000003,"d":"0.36"},{"v":2.1555362175198267,"d":"2.16"},{"v":2.1555362175198267,"d":"2.16"},{"v":0.7739888839999999,"d":"0.77"}]
["18029","Dearborn","IN",{"v":0.322696103,"d":"0.32"},{"v":2.212681880149827,"d":"2.21"},{"v":2.212681880149827,"d":"2.21"},{"v":0.8898854049999999,"d":"0.89"}]
["18031","Decatur","IN",{"v":0.348755419,"d":"0.35"},{"v":2.2733045822637394,"d":"2.27"},{"v":2.2733045822637394,"d":"2.27"},{"v":0.7794765195000001,"d":"0.78"}]
["18033","De Kalb","IN",{"v":0.327999601,"d":"0.33"},{"v":2.271618697764544,"d":"2.27"},{"v":2.271618697764544,"d":"2.27"},{"v":0.768582542,"d":"0.77"}]
["18035","Delaware","IN",{"v":0.30257775,"d":"0.30"},{"v":2.1471473592601527,"d":"2.15"},{"v":2.1471473592601527,"d":"2.15"},{"v":0.6956943839999999,"d":"0.70"}]
["18037","Dubois","IN",{"v":0.33380452,"d":"0.33"},{"v":2.151939735348482,"d":"2.15"},{"v":2.151939735348482,"d":"2.15"},{"v":0.8291046685,"d":"0.83"}]
["18039","Elkhart","IN",{"v":0.2798721089999999,"d":"0.28"},{"v":2.1488752960593023,"d":"2.15"},{"v":2.1488752960593023,"d":"2.15"},{"v":0.6983503235,"d":"0.70"}]
["18041","Fayette","IN",{"v":0.322858648,"d":"0.32"},{"v":2.2090526837988977,"d":"2.21"},{"v":2.2090526837988973,"d":"2.21"},{"v":0.7823866435000001,"d":"0.78"}]
["18043","Floyd","IN",{"v":0.267494029,"d":"0.27"},{"v":2.0870991214191963,"d":"2.09"},{"v":2.0870991214191967,"d":"2.09"},{"v":0.7673033664999999,"d":"0.77"}]
["18045","Fountain","IN",{"v":0.367876539,"d":"0.37"},{"v":2.27508616891475,"d":"2.28"},{"v":2.27508616891475,"d":"2.28"},{"v":0.8110280099999999,"d":"0.81"}]
["18047","Franklin","IN",{"v":0.368265091,"d":"0.37"},{"v":2.311820528902751,"d":"2.31"},{"v":2.311820528902751,"d":"2.31"},{"v":0.9293051829999999,"d":"0.93"}]
["18049","Fulton","IN",{"v":0.359694391,"d":"0.36"},{"v":2.3110716534959344,"d":"2.31"},{"v":2.311071653495934,"d":"2.31"},{"v":0.7947604914999999,"d":"0.79"}]
["18051","Gibson","IN",{"v":0.355035889,"d":"0.36"},{"v":2.1789825316526397,"d":"2.18"},{"v":2.1789825316526397,"d":"2.18"},{"v":0.7632031490000001,"d":"0.76"}]
["18053","Grant","IN",{"v":0.3240470670000001,"d":"0.32"},{"v":2.1859414243347985,"d":"2.19"},{"v":2.1859414243347985,"d":"2.19"},{"v":0.7120853525000003,"d":"0.71"}]
["18055","Greene","IN",{"v":0.358395574,"d":"0.36"},{"v":2.2298361971830163,"d":"2.23"},{"v":2.2298361971830163,"d":"2.23"},{"v":0.8653148475,"d":"0.87"}]
["18057","Hamilton","IN",{"v":0.250822443,"d":"0.25"},{"v":1.9746988463653663,"d":"1.97"},{"v":1.9746988463653663,"d":"1.97"},{"v":0.6183815914999999,"d":"0.62"}]
["18059","Hancock","IN",{"v":0.319247736,"d":"0.32"},{"v":2.1621283669375777,"d":"2.16"},{"v":2.1621283669375777,"d":"2.16"},{"v":0.7039345825,"d":"0.70"}]
["18061","Harrison","IN",{"v":0.363081579,"d":"0.36"},{"v":2.320004430822676,"d":"2.32"},{"v":2.320004430822676,"d":"2.32"},{"v":0.923451615,"d":"0.92"}]
["18063","Hendricks","IN",{"v":0.296183649,"d":"0.30"},{"v":2.187812651015999,"d":"2.19"},{"v":2.187812651015999,"d":"2.19"},{"v":0.6774285864999999,"d":"0.68"}]
["18065","Henry","IN",{"v":0.341057849,"d":"0.34"},{"v":2.2089051154289656,"d":"2.21"},{"v":2.2089051154289656,"d":"2.21"},{"v":0.745525465,"d":"0.75"}]
["18067","Howard","IN",{"v":0.308472632,"d":"0.31"},{"v":2.1338160648032964,"d":"2.13"},{"v":2.1338160648032964,"d":"2.13"},{"v":0.673864473,"d":"0.67"}]
["18069","Huntington","IN",{"v":0.348254549,"d":"0.35"},{"v":2.3031541783312837,"d":"2.30"},{"v":2.303154178331283,"d":"2.30"},{"v":0.7764048335,"d":"0.78"}]
["18071","Jackson","IN",{"v":0.33181450099999993,"d":"0.33"},{"v":2.262928214028395,"d":"2.26"},{"v":2.2629282140283955,"d":"2.26"},{"v":0.8202716965,"d":"0.82"}]
["18073","Jasper","IN",{"v":0.368395819,"d":"0.37"},{"v":2.288147645584308,"d":"2.29"},{"v":2.288147645584308,"d":"2.29"},{"v":0.7927469234999999,"d":"0.79"}]
["18075","Jay","IN",{"v":0.35885522799999997,"d":"0.36"},{"v":2.2556306281545035,"d":"2.26"},{"v":2.2556306281545035,"d":"2.26"},{"v":0.7628388155,"d":"0.76"}]
["18077","Jefferson","IN",{"v":0.330173855,"d":"0.33"},{"v":2.296640483277255,"d":"2.30"},{"v":2.2966404832772547,"d":"2.30"},{"v":0.8620965430000002,"d":"0.86"}]
["18079","Jennings","IN",{"v":0.344370612,"d":"0.34"},{"v":2.337868730746145,"d":"2.34"},{"v":2.3378687307461457,"d":"2.34"},{"v":0.8685444069999999,"d":"0.87"}]
["18081","Johnson","IN",{"v":0.280965747,"d":"0.28"},{"v":2.140222780592733,"d":"2.14"},{"v":2.140222780592733,"d":"2.14"},{"v":0.6775460065000001,"d":"0.68"}]
["18083","Knox","IN",{"v":0.343279902,"d":"0.34"},{"v":2.097400366451768,"d":"2.10"},{"v":2.097400366451768,"d":"2.10"},{"v":0.7330509635000001,"d":"0.73"}]
["18085","Kosciusko","IN",{"v":0.333853388,"d":"0.33"},{"v":2.25566316219056,"d":"2.26"},{"v":2.25566316219056,"d":"2.26"},{"v":0.7672775105,"d":"0.77"}]
["18087","Lagrange","IN",{"v":0.378465823,"d":"0.38"},{"v":2.3421294403145483,"d":"2.34"},{"v":2.3421294403145483,"d":"2.34"},{"v":0.8435521009999999,"d":"0.84"}]
["18089","Lake","IN",{"v":0.232459501,"d":"0.23"},{"v":1.7055877884729997,"d":"1.71"},{"v":1.7055877884730002,"d":"1.71"},{"v":0.6210817885,"d":"0.62"}]
["18091","La Porte","IN",{"v":0.317397233,"d":"0.32"},{"v":2.1873569048238366,"d":"2.19"},{"v":2.1873569048238366,"d":"2.19"},{"v":0.7628263114999999,"d":"0.76"}]
["18093","Lawrence","IN",{"v":0.3353305160000001,"d":"0.34"},{"v":2.2434805231549126,"d":"2.24"},{"v":2.2434805231549126,"d":"2.24"},{"v":0.8722759670000001,"d":"0.87"}]
["18095","Madison","IN",{"v":0.309965038,"d":"0.31"},{"v":2.137846345527149,"d":"2.14"},{"v":2.137846345527149,"d":"2.14"},{"v":0.6865571795,"d":"0.69"}]
["18097","Marion","IN",{"v":0.146003591,"d":"0.15"},{"v":0.0298496074846672,"d":"0.03"},{"v":0.029849607484667195,"d":"0.03"},{"v":0.541223881,"d":"0.54"}]
["18099","Marshall","IN",{"v":0.353736092,"d":"0.35"},{"v":2.2597902848755327,"d":"2.26"},{"v":2.2597902848755322,"d":"2.26"},{"v":0.7972214040000001,"d":"0.80"}]
["18101","Martin","IN",{"v":0.343405569,"d":"0.34"},{"v":2.273593254111116,"d":"2.27"},{"v":2.273593254111116,"d":"2.27"},{"v":0.9723885245,"d":"0.97"}]
["18103","Miami","IN",{"v":0.348074994,"d":"0.35"},{"v":2.290058371752048,"d":"2.29"},{"v":2.290058371752048,"d":"2.29"},{"v":0.775150814,"d":"0.78"}]
["18105","Monroe","IN",{"v":0.2671780100000001,"d":"0.27"},{"v":2.196150520146733,"d":"2.20"},{"v":2.1961505201467326,"d":"2.20"},{"v":0.8279279650000001,"d":"0.83"}]
["18107","Montgomery","IN",{"v":0.354345991,"d":"0.35"},{"v":2.2431753756254786,"d":"2.24"},{"v":2.2431753756254786,"d":"2.24"},{"v":0.7685138745,"d":"0.77"}]
["18109","Morgan","IN",{"v":0.326389956,"d":"0.33"},{"v":2.2937249825806854,"d":"2.29"},{"v":2.293724982580685,"d":"2.29"},{"v":0.8392525139999999,"d":"0.84"}]
["18111","Newton","IN",{"v":0.402202692,"d":"0.40"},{"v":2.301928661515744,"d":"2.30"},{"v":2.301928661515744,"d":"2.30"},{"v":0.8304805495000002,"d":"0.83"}]
["18113","Noble","IN",{"v":0.353679068,"d":"0.35"},{"v":2.3424810609756364,"d":"2.34"},{"v":2.3424810609756364,"d":"2.34"},{"v":0.8145683185000001,"d":"0.81"}]
["18115","Ohio","IN",{"v":0.37441372999999994,"d":"0.37"},{"v":2.306423343040505,"d":"2.31"},{"v":2.3064233430405046,"d":"2.31"},{"v":0.9633151189999998,"d":"0.96"}]
["18117","Orange","IN",{"v":0.358030658,"d":"0.36"},{"v":2.2919413412007907,"d":"2.29"},{"v":2.2919413412007916,"d":"2.29"},{"v":0.9365450269999999,"d":"0.94"}]
["18119","Owen","IN",{"v":0.36910403099999994,"d":"0.37"},{"v":2.435612740265483,"d":"2.44"},{"v":2.4356127402654835,"d":"2.44"},{"v":0.9765147610000001,"d":"0.98"}]
["18121","Parke","IN",{"v":0.362845893,"d":"0.36"},{"v":2.3641882604153914,"d":"2.36"},{"v":2.364188260415391,"d":"2.36"},{"v":0.9010423584999999,"d":"0.90"}]
["18123","Perry","IN",{"v":0.316897681,"d":"0.32"},{"v":2.221172273013897,"d":"2.22"},{"v":2.2211722730138965,"d":"2.22"},{"v":0.969810653,"d":"0.97"}]
["18125","Pike","IN",{"v":0.3905866150000001,"d":"0.39"},{"v":2.237220413848852,"d":"2.24"},{"v":2.237220413848852,"d":"2.24"},{"v":0.8933229705,"d":"0.89"}]
["18127","Porter","IN",{"v":0.289398148,"d":"0.29"},{"v":2.1512534176235807,"d":"2.15"},{"v":2.1512534176235807,"d":"2.15"},{"v":0.70822665,"d":"0.71"}]
["18129","Posey","IN",{"v":0.36628298500000006,"d":"0.37"},{"v":2.1634113623119053,"d":"2.16"},{"v":2.163411362311905,"d":"2.16"},{"v":0.796963924,"d":"0.80"}]
["18131","Pulaski","IN",{"v":0.37942310999999995,"d":"0.38"},{"v":2.3593018662890355,"d":"2.36"},{"v":2.3593018662890355,"d":"2.36"},{"v":0.8238013335,"d":"0.82"}]
["18133","Putnam","IN",{"v":0.350606773,"d":"0.35"},{"v":2.339196797893319,"d":"2.34"},{"v":2.339196797893319,"d":"2.34"},{"v":0.851564211,"d":"0.85"}]
["18135","Randolph","IN",{"v":0.365405123,"d":"0.37"},{"v":2.272294967615045,"d":"2.27"},{"v":2.272294967615045,"d":"2.27"},{"v":0.7707532100000001,"d":"0.77"}]
["18137","Ripley","IN",{"v":0.36696462299999993,"d":"0.37"},{"v":2.2621055501816723,"d":"2.26"},{"v":2.2621055501816723,"d":"2.26"},{"v":0.89681713,"d":"0.90"}]
["18139","Rush","IN",{"v":0.367541397,"d":"0.37"},{"v":2.2527090567662498,"d":"2.25"},{"v":2.2527090567662498,"d":"2.25"},{"v":0.7640013995000002,"d":"0.76"}]
["18141","St Joseph","IN",{"v":0.255583076,"d":"0.26"},{"v":2.075145390656677,"d":"2.08"},{"v":2.075145390656677,"d":"2.08"},{"v":0.6760726355000001,"d":"0.68"}]
["18143","Scott","IN",{"v":0.329218305,"d":"0.33"},{"v":2.2840405464660756,"d":"2.28"},{"v":2.284040546466076,"d":"2.28"},{"v":0.8444449399999999,"d":"0.84"}]
["18145","Shelby","IN",{"v":0.352889916,"d":"0.35"},{"v":2.2486137560833916,"d":"2.25"},{"v":2.248613756083391,"d":"2.25"},{"v":0.7453579505,"d":"0.75"}]
["18147","Spencer","IN",{"v":0.395637305,"d":"0.40"},{"v":2.182357948298926,"d":"2.18"},{"v":2.182357948298926,"d":"2.18"},{"v":0.8689978829999999,"d":"0.87"}]
["18149","Starke","IN",{"v":0.369106752,"d":"0.37"},{"v":2.276115831525318,"d":"2.28"},{"v":2.276115831525318,"d":"2.28"},{"v":0.8461439149999999,"d":"0.85"}]
["18151","Steuben","IN",{"v":0.34876101300000006,"d":"0.35"},{"v":2.311219511894306,"d":"2.31"},{"v":2.311219511894306,"d":"2.31"},{"v":0.8333206620000001,"d":"0.83"}]
["18153","Sullivan","IN",{"v":0.375637784,"d":"0.38"},{"v":2.2381958416046364,"d":"2.24"},{"v":2.2381958416046364,"d":"2.24"},{"v":0.816516916,"d":"0.82"}]
["18155","Switzerland","IN",{"v":0.370300237,"d":"0.37"},{"v":2.3661406803979266,"d":"2.37"},{"v":2.366140680397927,"d":"2.37"},{"v":0.9965113345,"d":"1.00"}]
["18157","Tippecanoe","IN",{"v":0.279249884,"d":"0.28"},{"v":2.157516178290794,"d":"2.16"},{"v":2.157516178290794,"d":"2.16"},{"v":0.6793363035,"d":"0.68"}]
["18159","Tipton","IN",{"v":0.373479971,"d":"0.37"},{"v":2.2543122475790653,"d":"2.25"},{"v":2.2543122475790653,"d":"2.25"},{"v":0.7528201599999998,"d":"0.75"}]
["18161","Union","IN",{"v":0.39126770299999997,"d":"0.39"},{"v":2.3681250678526466,"d":"2.37"},{"v":2.368125067852646,"d":"2.37"},{"v":0.8652612744999999,"d":"0.87"}]
["18163","Vanderburgh","IN",{"v":0.24576671200000003,"d":"0.25"},{"v":1.798023852320953,"d":"1.80"},{"v":1.798023852320953,"d":"1.80"},{"v":0.6513206374999999,"d":"0.65"}]
["18165","Vermillion","IN",{"v":0.350112875,"d":"0.35"},{"v":2.30169867583742,"d":"2.30"},{"v":2.30169867583742,"d":"2.30"},{"v":0.8176122135,"d":"0.82"}]
["18167","Vigo","IN",{"v":0.297376784,"d":"0.30"},{"v":2.2085956152582025,"d":"2.21"},{"v":2.2085956152582034,"d":"2.21"},{"v":0.747709523,"d":"0.75"}]
["18169","Wabash","IN",{"v":0.3467725629999999,"d":"0.35"},{"v":2.27660501680077,"d":"2.28"},{"v":2.27660501680077,"d":"2.28"},{"v":0.7773823900000001,"d":"0.78"}]
["18171","Warren","IN",{"v":0.383732919,"d":"0.38"},{"v":2.332781788573893,"d":"2.33"},{"v":2.332781788573893,"d":"2.33"},{"v":0.806577818,"d":"0.81"}]
["18173","Warrick","IN",{"v":0.316514866,"d":"0.32"},{"v":2.1355854533548255,"d":"2.14"},{"v":2.1355854533548255,"d":"2.14"},{"v":0.7750670705000001,"d":"0.78"}]
["18175","Washington","IN",{"v":0.363409651,"d":"0.36"},{"v":2.3192033885100094,"d":"2.32"},{"v":2.3192033885100094,"d":"2.32"},{"v":0.8823655349999998,"d":"0.88"}]
["18177","Wayne","IN",{"v":0.319161536,"d":"0.32"},{"v":2.1855507466971327,"d":"2.19"},{"v":2.1855507466971327,"d":"2.19"},{"v":0.7455671734999999,"d":"0.75"}]
["18179","Wells","IN",{"v":0.34761323400000005,"d":"0.35"},{"v":2.3125326791068304,"d":"2.31"},{"v":2.3125326791068304,"d":"2.31"},{"v":0.7547755400000001,"d":"0.75"}]
["18181","White","IN",{"v":0.36978621899999997,"d":"0.37"},{"v":2.2809255826539183,"d":"2.28"},{"v":2.2809255826539183,"d":"2.28"},{"v":0.7861178705,"d":"0.79"}]
["18183","Whitley","IN",{"v":0.36013715300000004,"d":"0.36"},{"v":2.315365012998415,"d":"2.32"},{"v":2.3153650129984147,"d":"2.32"},{"v":0.8035352945,"d":"0.80"}]
["19001","Adair","IA",{"v":0.296855397,"d":"0.30"},{"v":1.7189732255290888,"d":"1.72"},{"v":1.7189732255290888,"d":"1.72"},{"v":0.5983752210000001,"d":"0.60"}]
["19003","Adams","IA",{"v":0.292320466,"d":"0.29"},{"v":1.7334691314081188,"d":"1.73"},{"v":1.7334691314081188,"d":"1.73"},{"v":0.6038700565,"d":"0.60"}]
["19005","Allamakee","IA",{"v":0.24788683700000003,"d":"0.25"},{"v":1.8578556291487385,"d":"1.86"},{"v":1.8578556291487383,"d":"1.86"},{"v":0.6559877390000001,"d":"0.66"}]
["19007","Appanoose","IA",{"v":0.25453355,"d":"0.25"},{"v":1.736163224093114,"d":"1.74"},{"v":1.736163224093114,"d":"1.74"},{"v":0.588180278,"d":"0.59"}]
["19009","Audubon","IA",{"v":0.29282223499999993,"d":"0.29"},{"v":1.7529629461844891,"d":"1.75"},{"v":1.7529629461844893,"d":"1.75"},{"v":0.604800763,"d":"0.60"}]
["19011","Benton","IA",{"v":0.274566353,"d":"0.27"},{"v":1.719822585795353,"d":"1.72"},{"v":1.719822585795353,"d":"1.72"},{"v":0.586783078,"d":"0.59"}]
["19013","Black Hawk","IA",{"v":0.20868119499999999,"d":"0.21"},{"v":1.7053339128667302,"d":"1.71"},{"v":1.7053339128667302,"d":"1.71"},{"v":0.5070870815,"d":"0.51"}]
["19015","Boone","IA",{"v":0.246283814,"d":"0.25"},{"v":1.7277757020068651,"d":"1.73"},{"v":1.7277757020068654,"d":"1.73"},{"v":0.564975631,"d":"0.56"}]
["19017","Bremer","IA",{"v":0.258810247,"d":"0.26"},{"v":1.7682405926421458,"d":"1.77"},{"v":1.7682405926421458,"d":"1.77"},{"v":0.592932976,"d":"0.59"}]
["19019","Buchanan","IA",{"v":0.261963932,"d":"0.26"},{"v":1.7775224443328104,"d":"1.78"},{"v":1.7775224443328104,"d":"1.78"},{"v":0.5864709269999999,"d":"0.59"}]
["19021","Buena Vista","IA",{"v":0.24705309500000006,"d":"0.25"},{"v":1.7755530542741278,"d":"1.78"},{"v":1.7755530542741278,"d":"1.78"},{"v":0.56455153,"d":"0.56"}]
["19023","Butler","IA",{"v":0.283229326,"d":"0.28"},{"v":1.816408380180977,"d":"1.82"},{"v":1.816408380180977,"d":"1.82"},{"v":0.6238249695,"d":"0.62"}]
["19025","Calhoun","IA",{"v":0.291468249,"d":"0.29"},{"v":1.7514932852046434,"d":"1.75"},{"v":1.7514932852046434,"d":"1.75"},{"v":0.599479961,"d":"0.60"}]
["19027","Carroll","IA",{"v":0.254928307,"d":"0.25"},{"v":1.7415866055510176,"d":"1.74"},{"v":1.7415866055510176,"d":"1.74"},{"v":0.5529823424999999,"d":"0.55"}]
["19029","Cass","IA",{"v":0.257347371,"d":"0.26"},{"v":1.6619364980081028,"d":"1.66"},{"v":1.661936498008103,"d":"1.66"},{"v":0.553096193,"d":"0.55"}]
["19031","Cedar","IA",{"v":0.27766178,"d":"0.28"},{"v":1.7194375074005073,"d":"1.72"},{"v":1.7194375074005073,"d":"1.72"},{"v":0.5944044500000001,"d":"0.59"}]
["19033","Cerro Gordo","IA",{"v":0.22411068,"d":"0.22"},{"v":1.7525465117862635,"d":"1.75"},{"v":1.7525465117862635,"d":"1.75"},{"v":0.5202388975,"d":"0.52"}]
["19035","Cherokee","IA",{"v":0.255108629,"d":"0.26"},{"v":1.8043783076994493,"d":"1.80"},{"v":1.8043783076994497,"d":"1.80"},{"v":0.5802776184999999,"d":"0.58"}]
["19037","Chickasaw","IA",{"v":0.263467045,"d":"0.26"},{"v":1.804126376295142,"d":"1.80"},{"v":1.8041263762951418,"d":"1.80"},{"v":0.5956653435,"d":"0.60"}]
["19039","Clarke","IA",{"v":0.25026595,"d":"0.25"},{"v":1.7062657769033467,"d":"1.71"},{"v":1.7062657769033467,"d":"1.71"},{"v":0.5792896710000001,"d":"0.58"}]
["19041","Clay","IA",{"v":0.235519023,"d":"0.24"},{"v":1.7852256750759445,"d":"1.79"},{"v":1.7852256750759448,"d":"1.79"},{"v":0.541949173,"d":"0.54"}]
["19043","Clayton","IA",{"v":0.27167211999999996,"d":"0.27"},{"v":1.830760028085192,"d":"1.83"},{"v":1.830760028085192,"d":"1.83"},{"v":0.6645378820000001,"d":"0.66"}]
["19045","Clinton","IA",{"v":0.235391797,"d":"0.24"},{"v":1.6800320182445587,"d":"1.68"},{"v":1.6800320182445587,"d":"1.68"},{"v":0.5355788595000001,"d":"0.54"}]
["19047","Crawford","IA",{"v":0.254988868,"d":"0.25"},{"v":1.7676477586751063,"d":"1.77"},{"v":1.767647758675106,"d":"1.77"},{"v":0.5669159330000001,"d":"0.57"}]
["19049","Dallas","IA",{"v":0.23509604200000003,"d":"0.24"},{"v":1.7485599073623566,"d":"1.75"},{"v":1.7485599073623566,"d":"1.75"},{"v":0.5312526235000001,"d":"0.53"}]
["19051","Davis","IA",{"v":0.286566303,"d":"0.29"},{"v":1.7658522731830273,"d":"1.77"},{"v":1.765852273183027,"d":"1.77"},{"v":0.6293913494999998,"d":"0.63"}]
["19053","Decatur","IA",{"v":0.2847670030000001,"d":"0.28"},{"v":1.7411872642942698,"d":"1.74"},{"v":1.7411872642942698,"d":"1.74"},{"v":0.6301598835,"d":"0.63"}]
["19055","Delaware","IA",{"v":0.262103502,"d":"0.26"},{"v":1.7881872529388123,"d":"1.79"},{"v":1.7881872529388123,"d":"1.79"},{"v":0.598215102,"d":"0.60"}]
["19057","Des Moines","IA",{"v":0.228893209,"d":"0.23"},{"v":1.6567480237742847,"d":"1.66"},{"v":1.6567480237742849,"d":"1.66"},{"v":0.541823405,"d":"0.54"}]
["19059","Dickinson","IA",{"v":0.23553471700000003,"d":"0.24"},{"v":1.7980108507971913,"d":"1.80"},{"v":1.798010850797191,"d":"1.80"},{"v":0.5422437044999999,"d":"0.54"}]
["19061","Dubuque","IA",{"v":0.21946425000000003,"d":"0.22"},{"v":1.7158305259690116,"d":"1.72"},{"v":1.7158305259690119,"d":"1.72"},{"v":0.556709617,"d":"0.56"}]
["19063","Emmet","IA",{"v":0.244023133,"d":"0.24"},{"v":1.7832106611926446,"d":"1.78"},{"v":1.7832106611926446,"d":"1.78"},{"v":0.5530284929999999,"d":"0.55"}]
["19065","Fayette","IA",{"v":0.261032576,"d":"0.26"},{"v":1.787954299601304,"d":"1.79"},{"v":1.7879542996013043,"d":"1.79"},{"v":0.5996358440000001,"d":"0.60"}]
["19067","Floyd","IA",{"v":0.250648363,"d":"0.25"},{"v":1.7881577489172549,"d":"1.79"},{"v":1.7881577489172549,"d":"1.79"},{"v":0.5734847525000001,"d":"0.57"}]
["19069","Franklin","IA",{"v":0.25640872200000003,"d":"0.26"},{"v":1.8119690005977542,"d":"1.81"},{"v":1.8119690005977547,"d":"1.81"},{"v":0.5806784709999999,"d":"0.58"}]
["19071","Fremont","IA",{"v":0.2943174660000001,"d":"0.29"},{"v":1.7352364729641672,"d":"1.74"},{"v":1.7352364729641674,"d":"1.74"},{"v":0.6047554855,"d":"0.60"}]
["19073","Greene","IA",{"v":0.26080204799999995,"d":"0.26"},{"v":1.7405602760743109,"d":"1.74"},{"v":1.740560276074311,"d":"1.74"},{"v":0.5679757055,"d":"0.57"}]
["19075","Grundy","IA",{"v":0.2944037,"d":"0.29"},{"v":1.7426707844889502,"d":"1.74"},{"v":1.7426707844889497,"d":"1.74"},{"v":0.599179596,"d":"0.60"}]
["19077","Guthrie","IA",{"v":0.289825849,"d":"0.29"},{"v":1.7756008177858311,"d":"1.78"},{"v":1.775600817785831,"d":"1.78"},{"v":0.6189355994999999,"d":"0.62"}]
["19079","Hamilton","IA",{"v":0.252525458,"d":"0.25"},{"v":1.716417045645182,"d":"1.72"},{"v":1.7164170456451824,"d":"1.72"},{"v":0.5557489190000001,"d":"0.56"}]
["19081","Hancock","IA",{"v":0.264371103,"d":"0.26"},{"v":1.808793495063504,"d":"1.81"},{"v":1.808793495063504,"d":"1.81"},{"v":0.5854525020000001,"d":"0.59"}]
["19083","Hardin","IA",{"v":0.26923508,"d":"0.27"},{"v":1.7182718964674897,"d":"1.72"},{"v":1.7182718964674897,"d":"1.72"},{"v":0.5825163819999999,"d":"0.58"}]
["19085","Harrison","IA",{"v":0.27308053800000004,"d":"0.27"},{"v":1.7853658680703226,"d":"1.79"},{"v":1.7853658680703224,"d":"1.79"},{"v":0.604531439,"d":"0.60"}]
["19087","Henry","IA",{"v":0.262278733,"d":"0.26"},{"v":1.6872098882682576,"d":"1.69"},{"v":1.6872098882682578,"d":"1.69"},{"v":0.578547482,"d":"0.58"}]
["19089","Howard","IA",{"v":0.260704667,"d":"0.26"},{"v":1.8093581862686638,"d":"1.81"},{"v":1.8093581862686636,"d":"1.81"},{"v":0.5807193864999999,"d":"0.58"}]
["19091","Humboldt","IA",{"v":0.24624150299999994,"d":"0.25"},{"v":1.806091372427397,"d":"1.81"},{"v":1.8060913724273968,"d":"1.81"},{"v":0.560744658,"d":"0.56"}]
["19093","Ida","IA",{"v":0.290711648,"d":"0.29"},{"v":1.7537934076751336,"d":"1.75"},{"v":1.7537934076751338,"d":"1.75"},{"v":0.6027379440000001,"d":"0.60"}]
["19095","Iowa","IA",{"v":0.27203771700000007,"d":"0.27"},{"v":1.7036969130861481,"d":"1.70"},{"v":1.7036969130861481,"d":"1.70"},{"v":0.5993111485,"d":"0.60"}]
["19097","Jackson","IA",{"v":0.24799781,"d":"0.25"},{"v":1.735934579002942,"d":"1.74"},{"v":1.735934579002942,"d":"1.74"},{"v":0.596198472,"d":"0.60"}]
["19099","Jasper","IA",{"v":0.252417537,"d":"0.25"},{"v":1.7385918379595886,"d":"1.74"},{"v":1.7385918379595884,"d":"1.74"},{"v":0.564828651,"d":"0.56"}]
["19101","Jefferson","IA",{"v":0.244664619,"d":"0.24"},{"v":1.6927109835406955,"d":"1.69"},{"v":1.6927109835406953,"d":"1.69"},{"v":0.5587417910000001,"d":"0.56"}]
["19103","Johnson","IA",{"v":0.213331141,"d":"0.21"},{"v":1.689766746052567,"d":"1.69"},{"v":1.689766746052567,"d":"1.69"},{"v":0.5075347075,"d":"0.51"}]
["19105","Jones","IA",{"v":0.25897828799999995,"d":"0.26"},{"v":1.7459152544402303,"d":"1.75"},{"v":1.74591525444023,"d":"1.75"},{"v":0.583497963,"d":"0.58"}]
["19107","Keokuk","IA",{"v":0.29076169,"d":"0.29"},{"v":1.7294985193727856,"d":"1.73"},{"v":1.7294985193727859,"d":"1.73"},{"v":0.6095782815,"d":"0.61"}]
["19109","Kossuth","IA",{"v":0.25919588099999996,"d":"0.26"},{"v":1.802101305966514,"d":"1.80"},{"v":1.8021013059665139,"d":"1.80"},{"v":0.580193821,"d":"0.58"}]
["19111","Lee","IA",{"v":0.23880874500000002,"d":"0.24"},{"v":1.699536878708756,"d":"1.70"},{"v":1.699536878708756,"d":"1.70"},{"v":0.5776623805000001,"d":"0.58"}]
["19113","Linn","IA",{"v":0.20593390400000003,"d":"0.21"},{"v":1.6454746473990391,"d":"1.65"},{"v":1.6454746473990391,"d":"1.65"},{"v":0.49903906049999996,"d":"0.50"}]
["19115","Louisa","IA",{"v":0.288915179,"d":"0.29"},{"v":1.714991031532083,"d":"1.71"},{"v":1.714991031532083,"d":"1.71"},{"v":0.6153805984999999,"d":"0.62"}]
["19117","Lucas","IA",{"v":0.250780165,"d":"0.25"},{"v":1.731888364462686,"d":"1.73"},{"v":1.731888364462686,"d":"1.73"},{"v":0.5887261519999999,"d":"0.59"}]
["19119","Lyon","IA",{"v":0.2850608190000001,"d":"0.29"},{"v":1.8204505424633595,"d":"1.82"},{"v":1.8204505424633595,"d":"1.82"},{"v":0.613198981,"d":"0.61"}]
["19121","Madison","IA",{"v":0.263120622,"d":"0.26"},{"v":1.7121486340985368,"d":"1.71"},{"v":1.7121486340985368,"d":"1.71"},{"v":0.5909460265,"d":"0.59"}]
["19123","Mahaska","IA",{"v":0.248634023,"d":"0.25"},{"v":1.670137073801993,"d":"1.67"},{"v":1.6701370738019934,"d":"1.67"},{"v":0.549723824,"d":"0.55"}]
["19125","Marion","IA",{"v":0.24507824799999997,"d":"0.25"},{"v":1.6759510928819574,"d":"1.68"},{"v":1.6759510928819572,"d":"1.68"},{"v":0.563400505,"d":"0.56"}]
["19127","Marshall","IA",{"v":0.24010553500000004,"d":"0.24"},{"v":1.7110818567605015,"d":"1.71"},{"v":1.7110818567605013,"d":"1.71"},{"v":0.5381682575000001,"d":"0.54"}]
["19129","Mills","IA",{"v":0.26241495600000003,"d":"0.26"},{"v":1.7252785158589579,"d":"1.73"},{"v":1.7252785158589576,"d":"1.73"},{"v":0.5671341725,"d":"0.57"}]
["19131","Mitchell","IA",{"v":0.258970949,"d":"0.26"},{"v":1.8074524818535727,"d":"1.81"},{"v":1.8074524818535722,"d":"1.81"},{"v":0.5899851799999999,"d":"0.59"}]
["19133","Monona","IA",{"v":0.263312695,"d":"0.26"},{"v":1.7856698576849823,"d":"1.79"},{"v":1.7856698576849825,"d":"1.79"},{"v":0.5959079415,"d":"0.60"}]
["19135","Monroe","IA",{"v":0.24984278499999998,"d":"0.25"},{"v":1.7460177939506214,"d":"1.75"},{"v":1.7460177939506214,"d":"1.75"},{"v":0.6004630114999999,"d":"0.60"}]
["19137","Montgomery","IA",{"v":0.258298857,"d":"0.26"},{"v":1.6748017196042384,"d":"1.67"},{"v":1.6748017196042384,"d":"1.67"},{"v":0.5497814965,"d":"0.55"}]
["19139","Muscatine","IA",{"v":0.228594213,"d":"0.23"},{"v":1.6807505293457408,"d":"1.68"},{"v":1.6807505293457405,"d":"1.68"},{"v":0.531869379,"d":"0.53"}]
["19141","Obrien","IA",{"v":0.263113273,"d":"0.26"},{"v":1.7974763519678854,"d":"1.80"},{"v":1.7974763519678854,"d":"1.80"},{"v":0.5803063245000001,"d":"0.58"}]
["19143","Osceola","IA",{"v":0.259251077,"d":"0.26"},{"v":1.8186751908779866,"d":"1.82"},{"v":1.8186751908779866,"d":"1.82"},{"v":0.5716627485,"d":"0.57"}]
["19145","Page","IA",{"v":0.243799113,"d":"0.24"},{"v":1.6929965266793452,"d":"1.69"},{"v":1.692996526679345,"d":"1.69"},{"v":0.534389581,"d":"0.53"}]
["19147","Palo Alto","IA",{"v":0.256805944,"d":"0.26"},{"v":1.7933343555840424,"d":"1.79"},{"v":1.7933343555840424,"d":"1.79"},{"v":0.5780906634999999,"d":"0.58"}]
["19149","Plymouth","IA",{"v":0.257360908,"d":"0.26"},{"v":1.8076073495295262,"d":"1.81"},{"v":1.8076073495295262,"d":"1.81"},{"v":0.5793322155,"d":"0.58"}]
["19151","Pocahontas","IA",{"v":0.287992031,"d":"0.29"},{"v":1.8185991130777757,"d":"1.82"},{"v":1.8185991130777752,"d":"1.82"},{"v":0.611005994,"d":"0.61"}]
["19153","Polk","IA",{"v":0.170621558,"d":"0.17"},{"v":1.467568026803805,"d":"1.47"},{"v":1.467568026803805,"d":"1.47"},{"v":0.458070464,"d":"0.46"}]
["19155","Pottawattamie","IA",{"v":0.23035211900000002,"d":"0.23"},{"v":1.6430706482057824,"d":"1.64"},{"v":1.6430706482057824,"d":"1.64"},{"v":0.516743881,"d":"0.52"}]
["19157","Poweshiek","IA",{"v":0.255209588,"d":"0.26"},{"v":1.7321241402521281,"d":"1.73"},{"v":1.7321241402521277,"d":"1.73"},{"v":0.5650822710000001,"d":"0.57"}]
["19159","Ringgold","IA",{"v":0.291888908,"d":"0.29"},{"v":1.7579233117484883,"d":"1.76"},{"v":1.7579233117484885,"d":"1.76"},{"v":0.609039043,"d":"0.61"}]
["19161","Sac","IA",{"v":0.293757022,"d":"0.29"},{"v":1.762775667672515,"d":"1.76"},{"v":1.7627756676725155,"d":"1.76"},{"v":0.6006904025,"d":"0.60"}]
["19163","Scott","IA",{"v":0.20127796600000003,"d":"0.20"},{"v":1.6180147633526174,"d":"1.62"},{"v":1.6180147633526174,"d":"1.62"},{"v":0.496058732,"d":"0.50"}]
["19165","Shelby","IA",{"v":0.263303323,"d":"0.26"},{"v":1.768974049101611,"d":"1.77"},{"v":1.768974049101611,"d":"1.77"},{"v":0.5621348165000001,"d":"0.56"}]
["19167","Sioux","IA",{"v":0.255093753,"d":"0.26"},{"v":1.8119688995558836,"d":"1.81"},{"v":1.8119688995558838,"d":"1.81"},{"v":0.5642569085,"d":"0.56"}]
["19169","Story","IA",{"v":0.208152307,"d":"0.21"},{"v":1.6734012756848897,"d":"1.67"},{"v":1.6734012756848897,"d":"1.67"},{"v":0.5043081934999999,"d":"0.50"}]
["19171","Tama","IA",{"v":0.268261518,"d":"0.27"},{"v":1.7505754578084285,"d":"1.75"},{"v":1.7505754578084285,"d":"1.75"},{"v":0.5916217584999999,"d":"0.59"}]
["19173","Taylor","IA",{"v":0.293298848,"d":"0.29"},{"v":1.7537697428262267,"d":"1.75"},{"v":1.7537697428262264,"d":"1.75"},{"v":0.6080399949999999,"d":"0.61"}]
["19175","Union","IA",{"v":0.24445533700000002,"d":"0.24"},{"v":1.6927411083383537,"d":"1.69"},{"v":1.6927411083383537,"d":"1.69"},{"v":0.5458238120000001,"d":"0.55"}]
["19177","Van Buren","IA",{"v":0.287340964,"d":"0.29"},{"v":1.7847638198694222,"d":"1.78"},{"v":1.7847638198694222,"d":"1.78"},{"v":0.6390599105,"d":"0.64"}]
["19179","Wapello","IA",{"v":0.22953362799999996,"d":"0.23"},{"v":1.654223944390887,"d":"1.65"},{"v":1.654223944390887,"d":"1.65"},{"v":0.554075013,"d":"0.55"}]
["19181","Warren","IA",{"v":0.24237248,"d":"0.24"},{"v":1.7159259506784081,"d":"1.72"},{"v":1.7159259506784081,"d":"1.72"},{"v":0.5576338135,"d":"0.56"}]
["19183","Washington","IA",{"v":0.266841947,"d":"0.27"},{"v":1.7038217956817334,"d":"1.70"},{"v":1.703821795681733,"d":"1.70"},{"v":0.5789111105,"d":"0.58"}]
["19185","Wayne","IA",{"v":0.292819739,"d":"0.29"},{"v":1.7397984861804692,"d":"1.74"},{"v":1.739798486180469,"d":"1.74"},{"v":0.613672655,"d":"0.61"}]
["19187","Webster","IA",{"v":0.23870613900000007,"d":"0.24"},{"v":1.6954803381723471,"d":"1.70"},{"v":1.6954803381723473,"d":"1.70"},{"v":0.5415744365,"d":"0.54"}]
["19189","Winnebago","IA",{"v":0.264554845,"d":"0.26"},{"v":1.796857866188195,"d":"1.80"},{"v":1.796857866188195,"d":"1.80"},{"v":0.5848812419999999,"d":"0.58"}]
["19191","Winneshiek","IA",{"v":0.254495095,"d":"0.25"},{"v":1.804840090514202,"d":"1.80"},{"v":1.804840090514202,"d":"1.80"},{"v":0.6022185515,"d":"0.60"}]
["19193","Woodbury","IA",{"v":0.223949454,"d":"0.22"},{"v":1.7037977444579884,"d":"1.70"},{"v":1.7037977444579888,"d":"1.70"},{"v":0.5113260969999999,"d":"0.51"}]
["19195","Worth","IA",{"v":0.28467261,"d":"0.28"},{"v":1.8133723614119581,"d":"1.81"},{"v":1.813372361411958,"d":"1.81"},{"v":0.618505376,"d":"0.62"}]
["19197","Wright","IA",{"v":0.254936737,"d":"0.25"},{"v":1.7904631633011312,"d":"1.79"},{"v":1.790463163301131,"d":"1.79"},{"v":0.5745291955,"d":"0.57"}]
["20001","Allen","KS",{"v":0.371815437,"d":"0.37"},{"v":2.108554895633443,"d":"2.11"},{"v":2.108554895633443,"d":"2.11"},{"v":0.7570181559999999,"d":"0.76"}]
["20003","Anderson","KS",{"v":0.371649488,"d":"0.37"},{"v":2.236407125580963,"d":"2.24"},{"v":2.236407125580963,"d":"2.24"},{"v":0.765282938,"d":"0.77"}]
["20005","Atchison","KS",{"v":0.34096091400000006,"d":"0.34"},{"v":2.226172722769473,"d":"2.23"},{"v":2.2261727227694728,"d":"2.23"},{"v":0.7501834535,"d":"0.75"}]
["20007","Barber","KS",{"v":0.4201700890000001,"d":"0.42"},{"v":2.10946275481571,"d":"2.11"},{"v":2.1094627548157106,"d":"2.11"},{"v":0.8027309515000001,"d":"0.80"}]
["20009","Barton","KS",{"v":0.352768614,"d":"0.35"},{"v":2.110028560130563,"d":"2.11"},{"v":2.110028560130563,"d":"2.11"},{"v":0.7008675805000001,"d":"0.70"}]
["20011","Bourbon","KS",{"v":0.359023557,"d":"0.36"},{"v":2.1239237938571063,"d":"2.12"},{"v":2.123923793857106,"d":"2.12"},{"v":0.7638998659999999,"d":"0.76"}]
["20013","Brown","KS",{"v":0.37843122399999995,"d":"0.38"},{"v":2.2163217856830406,"d":"2.22"},{"v":2.2163217856830406,"d":"2.22"},{"v":0.7755410555000002,"d":"0.78"}]
["20015","Butler","KS",{"v":0.359898698,"d":"0.36"},{"v":2.124197767354192,"d":"2.12"},{"v":2.1241977673541923,"d":"2.12"},{"v":0.7132825874999998,"d":"0.71"}]
["20017","Chase","KS",{"v":0.42451329399999993,"d":"0.42"},{"v":2.2094841423861977,"d":"2.21"},{"v":2.2094841423861973,"d":"2.21"},{"v":0.7960162835000001,"d":"0.80"}]
["20019","Chautauqua","KS",{"v":0.41483992500000005,"d":"0.41"},{"v":2.1638489235593283,"d":"2.16"},{"v":2.1638489235593283,"d":"2.16"},{"v":0.8319461505,"d":"0.83"}]
["20021","Cherokee","KS",{"v":0.363308669,"d":"0.36"},{"v":2.182713020796096,"d":"2.18"},{"v":2.182713020796096,"d":"2.18"},{"v":0.7557967580000001,"d":"0.76"}]
["20023","Cheyenne","KS",{"v":0.42170058900000007,"d":"0.42"},{"v":2.2273281990960188,"d":"2.23"},{"v":2.2273281990960188,"d":"2.23"},{"v":0.7968414469999999,"d":"0.80"}]
["20025","Clark","KS",{"v":0.42854235200000007,"d":"0.43"},{"v":2.1173010058700026,"d":"2.12"},{"v":2.1173010058700026,"d":"2.12"},{"v":0.7807577545000001,"d":"0.78"}]
["20027","Clay","KS",{"v":0.35867197600000006,"d":"0.36"},{"v":2.238015190690049,"d":"2.24"},{"v":2.2380151906900494,"d":"2.24"},{"v":0.7445732325,"d":"0.74"}]
["20029","Cloud","KS",{"v":0.363984285,"d":"0.36"},{"v":2.207259093816154,"d":"2.21"},{"v":2.2072590938161545,"d":"2.21"},{"v":0.7382921574999998,"d":"0.74"}]
["20031","Coffey","KS",{"v":0.38460767399999995,"d":"0.38"},{"v":2.2249498964577867,"d":"2.22"},{"v":2.2249498964577876,"d":"2.22"},{"v":0.7743001715000001,"d":"0.77"}]
["20033","Comanche","KS",{"v":0.430468044,"d":"0.43"},{"v":2.159777866958071,"d":"2.16"},{"v":2.159777866958071,"d":"2.16"},{"v":0.7864918639999999,"d":"0.79"}]
["20035","Cowley","KS",{"v":0.351652996,"d":"0.35"},{"v":2.105291417082229,"d":"2.11"},{"v":2.1052914170822294,"d":"2.11"},{"v":0.7049174109999999,"d":"0.70"}]
["20037","Crawford","KS",{"v":0.34480648099999994,"d":"0.34"},{"v":2.088831510975146,"d":"2.09"},{"v":2.0888315109751465,"d":"2.09"},{"v":0.7248104135000001,"d":"0.72"}]
["20039","Decatur","KS",{"v":0.42195106299999996,"d":"0.42"},{"v":2.229610263400997,"d":"2.23"},{"v":2.229610263400997,"d":"2.23"},{"v":0.7998908884999999,"d":"0.80"}]
["20041","Dickinson","KS",{"v":0.382845773,"d":"0.38"},{"v":2.179766705265638,"d":"2.18"},{"v":2.179766705265638,"d":"2.18"},{"v":0.7574068134999999,"d":"0.76"}]
["20043","Doniphan","KS",{"v":0.378967477,"d":"0.38"},{"v":2.2597831596936624,"d":"2.26"},{"v":2.259783159693662,"d":"2.26"},{"v":0.8043212775,"d":"0.80"}]
["20045","Douglas","KS",{"v":0.299774293,"d":"0.30"},{"v":2.1133043610090025,"d":"2.11"},{"v":2.1133043610090025,"d":"2.11"},{"v":0.6876612315,"d":"0.69"}]
["20047","Edwards","KS",{"v":0.42503619,"d":"0.43"},{"v":2.1180577891469383,"d":"2.12"},{"v":2.1180577891469383,"d":"2.12"},{"v":0.7843303085,"d":"0.78"}]
["20049","Elk","KS",{"v":0.42003163300000007,"d":"0.42"},{"v":2.1158566061668225,"d":"2.12"},{"v":2.115856606166822,"d":"2.12"},{"v":0.8095612354999999,"d":"0.81"}]
["20051","Ellis","KS",{"v":0.344286696,"d":"0.34"},{"v":2.1182014385193417,"d":"2.12"},{"v":2.1182014385193417,"d":"2.12"},{"v":0.6840887380000001,"d":"0.68"}]
["20053","Ellsworth","KS",{"v":0.38275974099999993,"d":"0.38"},{"v":2.175231709930099,"d":"2.18"},{"v":2.175231709930099,"d":"2.18"},{"v":0.7539811064999999,"d":"0.75"}]
["20055","Finney","KS",{"v":0.34837574,"d":"0.35"},{"v":2.0804983007076348,"d":"2.08"},{"v":2.0804983007076343,"d":"2.08"},{"v":0.661366361,"d":"0.66"}]
["20057","Ford","KS",{"v":0.346030859,"d":"0.35"},{"v":2.090301445518173,"d":"2.09"},{"v":2.0903014455181728,"d":"2.09"},{"v":0.6731530595,"d":"0.67"}]
["20059","Franklin","KS",{"v":0.3556204680000001,"d":"0.36"},{"v":2.183589339952459,"d":"2.18"},{"v":2.183589339952459,"d":"2.18"},{"v":0.7713013190000001,"d":"0.77"}]
["20061","Geary","KS",{"v":0.32182743299999994,"d":"0.32"},{"v":2.150735939622157,"d":"2.15"},{"v":2.150735939622157,"d":"2.15"},{"v":0.6850399239999999,"d":"0.69"}]
["20063","Gove","KS",{"v":0.425783347,"d":"0.43"},{"v":2.2138240550369366,"d":"2.21"},{"v":2.2138240550369366,"d":"2.21"},{"v":0.7899068014999999,"d":"0.79"}]
["20065","Graham","KS",{"v":0.418816201,"d":"0.42"},{"v":2.19755741267318,"d":"2.20"},{"v":2.19755741267318,"d":"2.20"},{"v":0.8071462400000001,"d":"0.81"}]
["20067","Grant","KS",{"v":0.35021941,"d":"0.35"},{"v":2.1341683301353296,"d":"2.13"},{"v":2.13416833013533,"d":"2.13"},{"v":0.6652455155,"d":"0.67"}]
["20069","Gray","KS",{"v":0.42905206100000004,"d":"0.43"},{"v":2.120502093085982,"d":"2.12"},{"v":2.120502093085982,"d":"2.12"},{"v":0.7782804115,"d":"0.78"}]
["20071","Greeley","KS",{"v":0.4217557659999999,"d":"0.42"},{"v":2.214298122349983,"d":"2.21"},{"v":2.214298122349983,"d":"2.21"},{"v":0.7874067095,"d":"0.79"}]
["20073","Greenwood","KS",{"v":0.38574831400000004,"d":"0.39"},{"v":2.1655238162307686,"d":"2.17"},{"v":2.1655238162307686,"d":"2.17"},{"v":0.7503347960000001,"d":"0.75"}]
["20075","Hamilton","KS",{"v":0.429767869,"d":"0.43"},{"v":2.086621213008786,"d":"2.09"},{"v":2.086621213008786,"d":"2.09"},{"v":0.7805185309999999,"d":"0.78"}]
["20077","Harper","KS",{"v":0.429433349,"d":"0.43"},{"v":2.093646369191778,"d":"2.09"},{"v":2.093646369191778,"d":"2.09"},{"v":0.7853601459999999,"d":"0.79"}]
["20079","Harvey","KS",{"v":0.349020784,"d":"0.35"},{"v":2.0823563599518544,"d":"2.08"},{"v":2.0823563599518544,"d":"2.08"},{"v":0.6925967654999999,"d":"0.69"}]
["20081","Haskell","KS",{"v":0.42751750499999996,"d":"0.43"},{"v":2.1513581606980523,"d":"2.15"},{"v":2.1513581606980523,"d":"2.15"},{"v":0.780201907,"d":"0.78"}]
["20083","Hodgeman","KS",{"v":0.43167118899999996,"d":"0.43"},{"v":2.158111839230173,"d":"2.16"},{"v":2.1581118392301732,"d":"2.16"},{"v":0.781923092,"d":"0.78"}]
["20085","Jackson","KS",{"v":0.380826776,"d":"0.38"},{"v":2.3071339810171514,"d":"2.31"},{"v":2.3071339810171514,"d":"2.31"},{"v":0.8041694915,"d":"0.80"}]
["20087","Jefferson","KS",{"v":0.39898397300000005,"d":"0.40"},{"v":2.320961996715834,"d":"2.32"},{"v":2.320961996715834,"d":"2.32"},{"v":0.860183551,"d":"0.86"}]
["20089","Jewell","KS",{"v":0.4223845540000001,"d":"0.42"},{"v":2.2732683245640524,"d":"2.27"},{"v":2.273268324564052,"d":"2.27"},{"v":0.810405535,"d":"0.81"}]
["20091","Johnson","KS",{"v":0.219494247,"d":"0.22"},{"v":1.2109618965168967,"d":"1.21"},{"v":1.2109618965168967,"d":"1.21"},{"v":0.5954920905000001,"d":"0.60"}]
["20093","Kearny","KS",{"v":0.431658405,"d":"0.43"},{"v":2.0930362606371586,"d":"2.09"},{"v":2.0930362606371586,"d":"2.09"},{"v":0.782784571,"d":"0.78"}]
["20095","Kingman","KS",{"v":0.3824552440000001,"d":"0.38"},{"v":2.1661904188668104,"d":"2.17"},{"v":2.166190418866811,"d":"2.17"},{"v":0.7447309930000001,"d":"0.74"}]
["20097","Kiowa","KS",{"v":0.42575426000000005,"d":"0.43"},{"v":2.1471557233447367,"d":"2.15"},{"v":2.147155723344737,"d":"2.15"},{"v":0.7845556105,"d":"0.78"}]
["20099","Labette","KS",{"v":0.365831306,"d":"0.37"},{"v":2.1058990801322097,"d":"2.11"},{"v":2.1058990801322097,"d":"2.11"},{"v":0.7496649435,"d":"0.75"}]
["20101","Lane","KS",{"v":0.433739416,"d":"0.43"},{"v":2.2069078247399507,"d":"2.21"},{"v":2.2069078247399507,"d":"2.21"},{"v":0.785743287,"d":"0.79"}]
["20103","Leavenworth","KS",{"v":0.327018138,"d":"0.33"},{"v":2.224714291217622,"d":"2.22"},{"v":2.2247142912176225,"d":"2.22"},{"v":0.7621741165000001,"d":"0.76"}]
["20105","Lincoln","KS",{"v":0.421664035,"d":"0.42"},{"v":2.206329247229119,"d":"2.21"},{"v":2.206329247229119,"d":"2.21"},{"v":0.7955795305,"d":"0.80"}]
["20107","Linn","KS",{"v":0.405686544,"d":"0.41"},{"v":2.317309592900746,"d":"2.32"},{"v":2.317309592900746,"d":"2.32"},{"v":0.8587682444999999,"d":"0.86"}]
["20109","Logan","KS",{"v":0.42482974399999995,"d":"0.42"},{"v":2.1501156541361297,"d":"2.15"},{"v":2.1501156541361297,"d":"2.15"},{"v":0.7885836839999999,"d":"0.79"}]
["20111","Lyon","KS",{"v":0.338480084,"d":"0.34"},{"v":2.1739778933289813,"d":"2.17"},{"v":2.1739778933289813,"d":"2.17"},{"v":0.6978460375000001,"d":"0.70"}]
["20113","McPherson","KS",{"v":0.36455515499999996,"d":"0.36"},{"v":2.1485766094563306,"d":"2.15"},{"v":2.1485766094563306,"d":"2.15"},{"v":0.7237249124999999,"d":"0.72"}]
["20115","Marion","KS",{"v":0.40190057199999996,"d":"0.40"},{"v":2.1708679149146968,"d":"2.17"},{"v":2.1708679149146963,"d":"2.17"},{"v":0.778703504,"d":"0.78"}]
["20117","Marshall","KS",{"v":0.38107617,"d":"0.38"},{"v":2.2223775798889625,"d":"2.22"},{"v":2.2223775798889625,"d":"2.22"},{"v":0.7841818705,"d":"0.78"}]
["20119","Meade","KS",{"v":0.431722134,"d":"0.43"},{"v":2.1087313786722235,"d":"2.11"},{"v":2.108731378672223,"d":"2.11"},{"v":0.7793398555,"d":"0.78"}]
["20121","Miami","KS",{"v":0.36003422699999993,"d":"0.36"},{"v":2.2579854706378293,"d":"2.26"},{"v":2.2579854706378297,"d":"2.26"},{"v":0.7670632305000001,"d":"0.77"}]
["20123","Mitchell","KS",{"v":0.36834455699999996,"d":"0.37"},{"v":2.1935048564081865,"d":"2.19"},{"v":2.1935048564081865,"d":"2.19"},{"v":0.7398012370000001,"d":"0.74"}]
["20125","Montgomery","KS",{"v":0.35043407600000004,"d":"0.35"},{"v":2.0806598866321977,"d":"2.08"},{"v":2.0806598866321973,"d":"2.08"},{"v":0.7529424925,"d":"0.75"}]
["20127","Morris","KS",{"v":0.41990527,"d":"0.42"},{"v":2.2232707770331874,"d":"2.22"},{"v":2.2232707770331874,"d":"2.22"},{"v":0.798033874,"d":"0.80"}]
["20129","Morton","KS",{"v":0.43254473800000004,"d":"0.43"},{"v":2.145338680060834,"d":"2.15"},{"v":2.145338680060834,"d":"2.15"},{"v":0.7777905125000002,"d":"0.78"}]
["20131","Nemaha","KS",{"v":0.38814249200000006,"d":"0.39"},{"v":2.242421442330825,"d":"2.24"},{"v":2.2424214423308246,"d":"2.24"},{"v":0.7885975430000002,"d":"0.79"}]
["20133","Neosho","KS",{"v":0.36247215,"d":"0.36"},{"v":2.1094146373119305,"d":"2.11"},{"v":2.10941463731193,"d":"2.11"},{"v":0.740438134,"d":"0.74"}]
["20135","Ness","KS",{"v":0.422886406,"d":"0.42"},{"v":2.229426412177531,"d":"2.23"},{"v":2.229426412177531,"d":"2.23"},{"v":0.788368905,"d":"0.79"}]
["20137","Norton","KS",{"v":0.353368264,"d":"0.35"},{"v":2.237001197550942,"d":"2.24"},{"v":2.2370011975509425,"d":"2.24"},{"v":0.7249273325000001,"d":"0.72"}]
["20139","Osage","KS",{"v":0.394947183,"d":"0.39"},{"v":2.2387419706524274,"d":"2.24"},{"v":2.238741970652427,"d":"2.24"},{"v":0.80019235,"d":"0.80"}]
["20141","Osborne","KS",{"v":0.421633889,"d":"0.42"},{"v":2.1932987089690488,"d":"2.19"},{"v":2.1932987089690483,"d":"2.19"},{"v":0.8098505670000001,"d":"0.81"}]
["20143","Ottawa","KS",{"v":0.415510968,"d":"0.42"},{"v":2.3051769617979114,"d":"2.31"},{"v":2.3051769617979114,"d":"2.31"},{"v":0.8119312184999999,"d":"0.81"}]
["20145","Pawnee","KS",{"v":0.363684564,"d":"0.36"},{"v":2.0940334800710607,"d":"2.09"},{"v":2.0940334800710607,"d":"2.09"},{"v":0.689384517,"d":"0.69"}]
["20147","Phillips","KS",{"v":0.371417225,"d":"0.37"},{"v":2.229893073539679,"d":"2.23"},{"v":2.229893073539679,"d":"2.23"},{"v":0.745552229,"d":"0.75"}]
["20149","Pottawatomie","KS",{"v":0.368901719,"d":"0.37"},{"v":2.2426731630214847,"d":"2.24"},{"v":2.2426731630214842,"d":"2.24"},{"v":0.7801918964999999,"d":"0.78"}]
["20151","Pratt","KS",{"v":0.347994402,"d":"0.35"},{"v":2.076889841885448,"d":"2.08"},{"v":2.076889841885448,"d":"2.08"},{"v":0.6990909040000001,"d":"0.70"}]
["20153","Rawlins","KS",{"v":0.42521912799999995,"d":"0.43"},{"v":2.2612016732082414,"d":"2.26"},{"v":2.2612016732082414,"d":"2.26"},{"v":0.7957744525,"d":"0.80"}]
["20155","Reno","KS",{"v":0.349515519,"d":"0.35"},{"v":2.0698572162383044,"d":"2.07"},{"v":2.0698572162383044,"d":"2.07"},{"v":0.7002521174999999,"d":"0.70"}]
["20157","Republic","KS",{"v":0.414964202,"d":"0.41"},{"v":2.252075919732169,"d":"2.25"},{"v":2.252075919732169,"d":"2.25"},{"v":0.8086925905000001,"d":"0.81"}]
["20159","Rice","KS",{"v":0.38025928700000006,"d":"0.38"},{"v":2.1384533298281743,"d":"2.14"},{"v":2.1384533298281743,"d":"2.14"},{"v":0.754600817,"d":"0.75"}]
["20161","Riley","KS",{"v":0.307055385,"d":"0.31"},{"v":2.1902589521527327,"d":"2.19"},{"v":2.190258952152733,"d":"2.19"},{"v":0.7000080710000001,"d":"0.70"}]
["20163","Rooks","KS",{"v":0.4205268959999999,"d":"0.42"},{"v":2.2079583748803144,"d":"2.21"},{"v":2.2079583748803144,"d":"2.21"},{"v":0.8011762720000001,"d":"0.80"}]
["20165","Rush","KS",{"v":0.428130615,"d":"0.43"},{"v":2.169727100128686,"d":"2.17"},{"v":2.1697271001286857,"d":"2.17"},{"v":0.7845907255000001,"d":"0.78"}]
["20167","Russell","KS",{"v":0.363699913,"d":"0.36"},{"v":2.152602444248219,"d":"2.15"},{"v":2.152602444248219,"d":"2.15"},{"v":0.7155628209999999,"d":"0.72"}]
["20169","Saline","KS",{"v":0.33415036900000006,"d":"0.33"},{"v":2.1170854866786457,"d":"2.12"},{"v":2.1170854866786457,"d":"2.12"},{"v":0.668383498,"d":"0.67"}]
["20171","Scott","KS",{"v":0.3529148879999999,"d":"0.35"},{"v":2.1732988246925853,"d":"2.17"},{"v":2.1732988246925853,"d":"2.17"},{"v":0.6788171039999998,"d":"0.68"}]
["20173","Sedgwick","KS",{"v":0.280830522,"d":"0.28"},{"v":1.9861935021074884,"d":"1.99"},{"v":1.9861935021074884,"d":"1.99"},{"v":0.6184785295,"d":"0.62"}]
["20175","Seward","KS",{"v":0.33594677,"d":"0.34"},{"v":2.0726630805067408,"d":"2.07"},{"v":2.0726630805067408,"d":"2.07"},{"v":0.646119958,"d":"0.65"}]
["20177","Shawnee","KS",{"v":0.29495254699999995,"d":"0.29"},{"v":2.0871522961579494,"d":"2.09"},{"v":2.0871522961579494,"d":"2.09"},{"v":0.674557289,"d":"0.67"}]
["20179","Sheridan","KS",{"v":0.41961811199999993,"d":"0.42"},{"v":2.2403761574029915,"d":"2.24"},{"v":2.2403761574029915,"d":"2.24"},{"v":0.795663613,"d":"0.80"}]
["20181","Sherman","KS",{"v":0.341745024,"d":"0.34"},{"v":2.1523310792583374,"d":"2.15"},{"v":2.1523310792583374,"d":"2.15"},{"v":0.6910007610000001,"d":"0.69"}]
["20183","Smith","KS",{"v":0.423213903,"d":"0.42"},{"v":2.2368139967528156,"d":"2.24"},{"v":2.236813996752816,"d":"2.24"},{"v":0.8038497345,"d":"0.80"}]
["20185","Stafford","KS",{"v":0.427010644,"d":"0.43"},{"v":2.109269614132713,"d":"2.11"},{"v":2.109269614132713,"d":"2.11"},{"v":0.794785382,"d":"0.79"}]
["20187","Stanton","KS",{"v":0.427918366,"d":"0.43"},{"v":2.1471625935423426,"d":"2.15"},{"v":2.1471625935423426,"d":"2.15"},{"v":0.7824340204999999,"d":"0.78"}]
["20189","Stevens","KS",{"v":0.357078725,"d":"0.36"},{"v":2.1362994326587192,"d":"2.14"},{"v":2.1362994326587192,"d":"2.14"},{"v":0.6846171280000001,"d":"0.68"}]
["20191","Sumner","KS",{"v":0.384927892,"d":"0.38"},{"v":2.140349524608389,"d":"2.14"},{"v":2.140349524608389,"d":"2.14"},{"v":0.7445110045,"d":"0.74"}]
["20193","Thomas","KS",{"v":0.358279453,"d":"0.36"},{"v":2.1990866486330507,"d":"2.20"},{"v":2.1990866486330507,"d":"2.20"},{"v":0.7010276260000001,"d":"0.70"}]
["20195","Trego","KS",{"v":0.421829687,"d":"0.42"},{"v":2.1948101188350555,"d":"2.19"},{"v":2.1948101188350555,"d":"2.19"},{"v":0.7892299475000001,"d":"0.79"}]
["20197","Wabaunsee","KS",{"v":0.42337312600000004,"d":"0.42"},{"v":2.2433474791633676,"d":"2.24"},{"v":2.2433474791633676,"d":"2.24"},{"v":0.8011253085,"d":"0.80"}]
["20199","Wallace","KS",{"v":0.42504878799999996,"d":"0.43"},{"v":2.202781789270045,"d":"2.20"},{"v":2.2027817892700456,"d":"2.20"},{"v":0.790005668,"d":"0.79"}]
["20201","Washington","KS",{"v":0.41567527300000007,"d":"0.42"},{"v":2.2291504269516866,"d":"2.23"},{"v":2.2291504269516866,"d":"2.23"},{"v":0.8163120245000001,"d":"0.82"}]
["20203","Wichita","KS",{"v":0.428638626,"d":"0.43"},{"v":2.1820165148629314,"d":"2.18"},{"v":2.182016514862932,"d":"2.18"},{"v":0.788656639,"d":"0.79"}]
["20205","Wilson","KS",{"v":0.389083154,"d":"0.39"},{"v":2.1424281643254393,"d":"2.14"},{"v":2.1424281643254393,"d":"2.14"},{"v":0.7909172215,"d":"0.79"}]
["20207","Woodson","KS",{"v":0.42554067399999995,"d":"0.43"},{"v":2.170694925691157,"d":"2.17"},{"v":2.1706949256911576,"d":"2.17"},{"v":0.8072640809999999,"d":"0.81"}]
["20209","Wyandotte","KS",{"v":0.22593453700000002,"d":"0.23"},{"v":1.643596483165781,"d":"1.64"},{"v":1.6435964831657812,"d":"1.64"},{"v":0.6479037744999999,"d":"0.65"}]
["21001","Adair","KY",{"v":0.4638017039999999,"d":"0.46"},{"v":2.9898943132215683,"d":"2.99"},{"v":2.9898943132215683,"d":"2.99"},{"v":1.2248914669999997,"d":"1.22"}]
["21003","Allen","KY",{"v":0.4695526769999999,"d":"0.47"},{"v":2.9647139291307574,"d":"2.96"},{"v":2.9647139291307574,"d":"2.96"},{"v":1.1699999875000004,"d":"1.17"}]
["21005","Anderson","KY",{"v":0.41604019099999995,"d":"0.42"},{"v":2.8693227030223722,"d":"2.87"},{"v":2.8693227030223722,"d":"2.87"},{"v":1.1473493085000002,"d":"1.15"}]
["21007","Ballard","KY",{"v":0.5316925780000001,"d":"0.53"},{"v":2.8682416517821845,"d":"2.87"},{"v":2.8682416517821845,"d":"2.87"},{"v":1.0909958690000001,"d":"1.09"}]
["21009","Barren","KY",{"v":0.4666829760000001,"d":"0.47"},{"v":2.7740772769127915,"d":"2.77"},{"v":2.7740772769127915,"d":"2.77"},{"v":1.066563998,"d":"1.07"}]
["21011","Bath","KY",{"v":0.48439135400000005,"d":"0.48"},{"v":3.051349536910311,"d":"3.05"},{"v":3.0513495369103114,"d":"3.05"},{"v":1.246384612,"d":"1.25"}]
["21013","Bell","KY",{"v":0.399954134,"d":"0.40"},{"v":3.000227001363101,"d":"3.00"},{"v":3.000227001363101,"d":"3.00"},{"v":1.4733308405,"d":"1.47"}]
["21015","Boone","KY",{"v":0.33794282700000006,"d":"0.34"},{"v":2.73670755586416,"d":"2.74"},{"v":2.7367075558641596,"d":"2.74"},{"v":0.9902237850000001,"d":"0.99"}]
["21017","Bourbon","KY",{"v":0.468894554,"d":"0.47"},{"v":2.8105051042210487,"d":"2.81"},{"v":2.8105051042210487,"d":"2.81"},{"v":0.958469044,"d":"0.96"}]
["21019","Boyd","KY",{"v":0.354895858,"d":"0.35"},{"v":2.749828537027647,"d":"2.75"},{"v":2.749828537027647,"d":"2.75"},{"v":1.1938986729999999,"d":"1.19"}]
["21021","Boyle","KY",{"v":0.416436309,"d":"0.42"},{"v":2.734524340677756,"d":"2.73"},{"v":2.734524340677756,"d":"2.73"},{"v":1.042778331,"d":"1.04"}]
["21023","Bracken","KY",{"v":0.4802532679999999,"d":"0.48"},{"v":2.969645328727839,"d":"2.97"},{"v":2.9696453287278386,"d":"2.97"},{"v":1.2902647395000002,"d":"1.29"}]
["21025","Breathitt","KY",{"v":0.418800698,"d":"0.42"},{"v":3.1345643195145545,"d":"3.13"},{"v":3.1345643195145545,"d":"3.13"},{"v":1.5291984520000002,"d":"1.53"}]
["21027","Breckinridge","KY",{"v":0.492458443,"d":"0.49"},{"v":2.9564423039645535,"d":"2.96"},{"v":2.956442303964553,"d":"2.96"},{"v":1.2454722735000001,"d":"1.25"}]
["21029","Bullitt","KY",{"v":0.381497794,"d":"0.38"},{"v":2.766255490162144,"d":"2.77"},{"v":2.766255490162144,"d":"2.77"},{"v":1.1622829110000001,"d":"1.16"}]
["21031","Butler","KY",{"v":0.487701561,"d":"0.49"},{"v":2.9377218569404455,"d":"2.94"},{"v":2.9377218569404455,"d":"2.94"},{"v":1.280488084,"d":"1.28"}]
["21033","Caldwell","KY",{"v":0.44049528500000007,"d":"0.44"},{"v":2.8412234491247172,"d":"2.84"},{"v":2.841223449124718,"d":"2.84"},{"v":1.1440560775,"d":"1.14"}]
["21035","Calloway","KY",{"v":0.434921274,"d":"0.43"},{"v":2.7563762287237985,"d":"2.76"},{"v":2.7563762287237985,"d":"2.76"},{"v":1.091347521,"d":"1.09"}]
["21037","Campbell","KY",{"v":0.3177668,"d":"0.32"},{"v":2.538613662940369,"d":"2.54"},{"v":2.538613662940369,"d":"2.54"},{"v":1.031201476,"d":"1.03"}]
["21039","Carlisle","KY",{"v":0.5284950889999999,"d":"0.53"},{"v":2.862244859183739,"d":"2.86"},{"v":2.8622448591837384,"d":"2.86"},{"v":1.1061610815,"d":"1.11"}]
["21041","Carroll","KY",{"v":0.42293640500000007,"d":"0.42"},{"v":2.880428230738605,"d":"2.88"},{"v":2.880428230738605,"d":"2.88"},{"v":1.1802284334999997,"d":"1.18"}]
["21043","Carter","KY",{"v":0.428517517,"d":"0.43"},{"v":3.116471168738881,"d":"3.12"},{"v":3.1164711687388813,"d":"3.12"},{"v":1.4135006595000001,"d":"1.41"}]
["21045","Casey","KY",{"v":0.48331828399999993,"d":"0.48"},{"v":3.049565379973637,"d":"3.05"},{"v":3.0495653799736373,"d":"3.05"},{"v":1.303324819,"d":"1.30"}]
["21047","Christian","KY",{"v":0.423660478,"d":"0.42"},{"v":2.697608209019166,"d":"2.70"},{"v":2.697608209019166,"d":"2.70"},{"v":1.0339932575,"d":"1.03"}]
["21049","Clark","KY",{"v":0.42067647299999994,"d":"0.42"},{"v":2.793474792377162,"d":"2.79"},{"v":2.793474792377162,"d":"2.79"},{"v":0.9882420895,"d":"0.99"}]
["21051","Clay","KY",{"v":0.42736617300000007,"d":"0.43"},{"v":3.024609391047886,"d":"3.02"},{"v":3.0246093910478855,"d":"3.02"},{"v":1.5256170180000002,"d":"1.53"}]
["21053","Clinton","KY",{"v":0.4803805850000001,"d":"0.48"},{"v":3.0663327997821073,"d":"3.07"},{"v":3.066332799782107,"d":"3.07"},{"v":1.3007816175,"d":"1.30"}]
["21055","Crittenden","KY",{"v":0.469933777,"d":"0.47"},{"v":2.91474432473793,"d":"2.91"},{"v":2.91474432473793,"d":"2.91"},{"v":1.162707089,"d":"1.16"}]
["21057","Cumberland","KY",{"v":0.471530194,"d":"0.47"},{"v":2.9926346622493702,"d":"2.99"},{"v":2.9926346622493702,"d":"2.99"},{"v":1.4271463970000002,"d":"1.43"}]
["21059","Daviess","KY",{"v":0.412084673,"d":"0.41"},{"v":2.607423884622976,"d":"2.61"},{"v":2.6074238846229756,"d":"2.61"},{"v":0.938792599,"d":"0.94"}]
["21061","Edmonson","KY",{"v":0.479554833,"d":"0.48"},{"v":3.0661295197479177,"d":"3.07"},{"v":3.0661295197479177,"d":"3.07"},{"v":1.3133467564999999,"d":"1.31"}]
["21063","Elliott","KY",{"v":0.44860529,"d":"0.45"},{"v":3.1966379688266615,"d":"3.20"},{"v":3.1966379688266606,"d":"3.20"},{"v":1.499032058,"d":"1.50"}]
["21065","Estill","KY",{"v":0.434461625,"d":"0.43"},{"v":2.9702326056010477,"d":"2.97"},{"v":2.9702326056010477,"d":"2.97"},{"v":1.3759799714999998,"d":"1.38"}]
["21067","Fayette","KY",{"v":0.28806373499999993,"d":"0.29"},{"v":1.7078372526861358,"d":"1.71"},{"v":1.7078372526861363,"d":"1.71"},{"v":0.7753873029999999,"d":"0.78"}]
["21069","Fleming","KY",{"v":0.46765947,"d":"0.47"},{"v":3.0505336674281907,"d":"3.05"},{"v":3.05053366742819,"d":"3.05"},{"v":1.1828751190000002,"d":"1.18"}]
["21071","Floyd","KY",{"v":0.4242249189999999,"d":"0.42"},{"v":2.984916248928503,"d":"2.98"},{"v":2.9849162489285033,"d":"2.98"},{"v":1.4585291089999999,"d":"1.46"}]
["21073","Franklin","KY",{"v":0.38435127700000005,"d":"0.38"},{"v":2.7107466010029437,"d":"2.71"},{"v":2.7107466010029437,"d":"2.71"},{"v":1.0678412695000004,"d":"1.07"}]
["21075","Fulton","KY",{"v":0.4830522950000001,"d":"0.48"},{"v":2.683394652167709,"d":"2.68"},{"v":2.683394652167709,"d":"2.68"},{"v":1.033646911,"d":"1.03"}]
["21077","Gallatin","KY",{"v":0.467459319,"d":"0.47"},{"v":3.0891835665030007,"d":"3.09"},{"v":3.089183566503,"d":"3.09"},{"v":1.2607721815,"d":"1.26"}]
["21079","Garrard","KY",{"v":0.48104438399999994,"d":"0.48"},{"v":2.9863619499553518,"d":"2.99"},{"v":2.9863619499553518,"d":"2.99"},{"v":1.1382155884999998,"d":"1.14"}]
["21081","Grant","KY",{"v":0.432966458,"d":"0.43"},{"v":2.9600088510458344,"d":"2.96"},{"v":2.9600088510458344,"d":"2.96"},{"v":1.2205109645,"d":"1.22"}]
["21083","Graves","KY",{"v":0.4808108930000001,"d":"0.48"},{"v":2.787637816241686,"d":"2.79"},{"v":2.787637816241686,"d":"2.79"},{"v":1.0655980755,"d":"1.07"}]
["21085","Grayson","KY",{"v":0.460474442,"d":"0.46"},{"v":2.9679162460139197,"d":"2.97"},{"v":2.9679162460139197,"d":"2.97"},{"v":1.2029313405,"d":"1.20"}]
["21087","Green","KY",{"v":0.50681528,"d":"0.51"},{"v":2.9150683591798288,"d":"2.92"},{"v":2.9150683591798283,"d":"2.92"},{"v":1.1972990040000002,"d":"1.20"}]
["21089","Greenup","KY",{"v":0.393560771,"d":"0.39"},{"v":2.8519974464708726,"d":"2.85"},{"v":2.8519974464708726,"d":"2.85"},{"v":1.2743388189999998,"d":"1.27"}]
["21091","Hancock","KY",{"v":0.474702959,"d":"0.47"},{"v":2.8417905096350338,"d":"2.84"},{"v":2.8417905096350338,"d":"2.84"},{"v":1.244018069,"d":"1.24"}]
["21093","Hardin","KY",{"v":0.407348942,"d":"0.41"},{"v":2.8503229178939,"d":"2.85"},{"v":2.8503229178939,"d":"2.85"},{"v":1.069198128,"d":"1.07"}]
["21095","Harlan","KY",{"v":0.39705007299999995,"d":"0.40"},{"v":3.106314219859666,"d":"3.11"},{"v":3.106314219859666,"d":"3.11"},{"v":1.4676582885,"d":"1.47"}]
["21097","Harrison","KY",{"v":0.461930078,"d":"0.46"},{"v":2.870303300208278,"d":"2.87"},{"v":2.8703033002082785,"d":"2.87"},{"v":1.109164815,"d":"1.11"}]
["21099","Hart","KY",{"v":0.477410701,"d":"0.48"},{"v":2.9499525485544726,"d":"2.95"},{"v":2.9499525485544726,"d":"2.95"},{"v":1.2200901815,"d":"1.22"}]
["21101","Henderson","KY",{"v":0.437467338,"d":"0.44"},{"v":2.685263365709805,"d":"2.69"},{"v":2.6852633657098055,"d":"2.69"},{"v":0.9611994615,"d":"0.96"}]
["21103","Henry","KY",{"v":0.503838396,"d":"0.50"},{"v":2.9570397291439043,"d":"2.96"},{"v":2.957039729143905,"d":"2.96"},{"v":1.1904041965,"d":"1.19"}]
["21105","Hickman","KY",{"v":0.530904236,"d":"0.53"},{"v":2.870616202011774,"d":"2.87"},{"v":2.8706162020117745,"d":"2.87"},{"v":1.1028986305000001,"d":"1.10"}]
["21107","Hopkins","KY",{"v":0.4308774149999999,"d":"0.43"},{"v":2.7634970654564786,"d":"2.76"},{"v":2.7634970654564786,"d":"2.76"},{"v":1.1223611374999998,"d":"1.12"}]
["21109","Jackson","KY",{"v":0.45784418,"d":"0.46"},{"v":3.089208176447236,"d":"3.09"},{"v":3.089208176447236,"d":"3.09"},{"v":1.474958197,"d":"1.47"}]
["21111","Jefferson","KY",{"v":0.21123709199999996,"d":"0.21"},{"v":0.10844176691731121,"d":"0.11"},{"v":0.1084417669173112,"d":"0.11"},{"v":0.785929134,"d":"0.79"}]
["21113","Jessamine","KY",{"v":0.40763314,"d":"0.41"},{"v":2.777355351367739,"d":"2.78"},{"v":2.7773553513677394,"d":"2.78"},{"v":0.9699084490000001,"d":"0.97"}]
["21115","Johnson","KY",{"v":0.408393328,"d":"0.41"},{"v":3.0543308580080297,"d":"3.05"},{"v":3.0543308580080297,"d":"3.05"},{"v":1.4537815305,"d":"1.45"}]
["21117","Kenton","KY",{"v":0.2824842470000001,"d":"0.28"},{"v":2.029356195790557,"d":"2.03"},{"v":2.029356195790557,"d":"2.03"},{"v":0.9442234035,"d":"0.94"}]
["21119","Knott","KY",{"v":0.448765767,"d":"0.45"},{"v":2.9848414369710845,"d":"2.98"},{"v":2.9848414369710845,"d":"2.98"},{"v":1.4981496805000003,"d":"1.50"}]
["21121","Knox","KY",{"v":0.40578642000000004,"d":"0.41"},{"v":3.0165625906089186,"d":"3.02"},{"v":3.0165625906089186,"d":"3.02"},{"v":1.4160914709999999,"d":"1.42"}]
["21123","Larue","KY",{"v":0.478430432,"d":"0.48"},{"v":2.896175005740424,"d":"2.90"},{"v":2.896175005740424,"d":"2.90"},{"v":1.1572128554999999,"d":"1.16"}]
["21125","Laurel","KY",{"v":0.40850340999999996,"d":"0.41"},{"v":3.0176102888540943,"d":"3.02"},{"v":3.017610288854094,"d":"3.02"},{"v":1.2605169805,"d":"1.26"}]
["21127","Lawrence","KY",{"v":0.42388078599999995,"d":"0.42"},{"v":3.0980579088366844,"d":"3.10"},{"v":3.0980579088366844,"d":"3.10"},{"v":1.4588324019999999,"d":"1.46"}]
["21129","Lee","KY",{"v":0.44437317900000006,"d":"0.44"},{"v":3.1066583891001534,"d":"3.11"},{"v":3.106658389100154,"d":"3.11"},{"v":1.531523753,"d":"1.53"}]
["21131","Leslie","KY",{"v":0.44598177599999994,"d":"0.45"},{"v":3.2250544409062543,"d":"3.23"},{"v":3.2250544409062543,"d":"3.23"},{"v":1.5794504325,"d":"1.58"}]
["21133","Letcher","KY",{"v":0.44711471,"d":"0.45"},{"v":3.112148612947097,"d":"3.11"},{"v":3.112148612947097,"d":"3.11"},{"v":1.5076406249999998,"d":"1.51"}]
["21135","Lewis","KY",{"v":0.462678025,"d":"0.46"},{"v":3.07105079854324,"d":"3.07"},{"v":3.07105079854324,"d":"3.07"},{"v":1.4331950120000003,"d":"1.43"}]
["21137","Lincoln","KY",{"v":0.475307879,"d":"0.48"},{"v":3.0029009191304907,"d":"3.00"},{"v":3.0029009191304907,"d":"3.00"},{"v":1.173662151,"d":"1.17"}]
["21139","Livingston","KY",{"v":0.49647980799999997,"d":"0.50"},{"v":2.9411601692473166,"d":"2.94"},{"v":2.9411601692473166,"d":"2.94"},{"v":1.206980638,"d":"1.21"}]
["21141","Logan","KY",{"v":0.48831070899999995,"d":"0.49"},{"v":2.806524655313584,"d":"2.81"},{"v":2.8065246553135834,"d":"2.81"},{"v":1.0942372105,"d":"1.09"}]
["21143","Lyon","KY",{"v":0.4958210830000001,"d":"0.50"},{"v":2.9193237587051053,"d":"2.92"},{"v":2.9193237587051057,"d":"2.92"},{"v":1.2548535075,"d":"1.25"}]
["21145","McCracken","KY",{"v":0.39833196099999996,"d":"0.40"},{"v":2.671915249534908,"d":"2.67"},{"v":2.6719152495349077,"d":"2.67"},{"v":0.9677408979999998,"d":"0.97"}]
["21147","McCreary","KY",{"v":0.44999582900000007,"d":"0.45"},{"v":3.13431680046184,"d":"3.13"},{"v":3.13431680046184,"d":"3.13"},{"v":1.566108224,"d":"1.57"}]
["21149","Mclean","KY",{"v":0.52294306,"d":"0.52"},{"v":2.8837747083279575,"d":"2.88"},{"v":2.883774708327957,"d":"2.88"},{"v":1.097031573,"d":"1.10"}]
["21151","Madison","KY",{"v":0.402923275,"d":"0.40"},{"v":2.850123130021795,"d":"2.85"},{"v":2.850123130021795,"d":"2.85"},{"v":1.0687055435,"d":"1.07"}]
["21153","Magoffin","KY",{"v":0.433330532,"d":"0.43"},{"v":3.172934233903821,"d":"3.17"},{"v":3.1729342339038205,"d":"3.17"},{"v":1.5288326694999999,"d":"1.53"}]
["21155","Marion","KY",{"v":0.4651579370000001,"d":"0.47"},{"v":2.8784377577270615,"d":"2.88"},{"v":2.8784377577270615,"d":"2.88"},{"v":1.1588135384999998,"d":"1.16"}]
["21157","Marshall","KY",{"v":0.478576428,"d":"0.48"},{"v":2.793803361728883,"d":"2.79"},{"v":2.7938033617288833,"d":"2.79"},{"v":1.1710506484999998,"d":"1.17"}]
["21159","Martin","KY",{"v":0.450414518,"d":"0.45"},{"v":3.0492066800021314,"d":"3.05"},{"v":3.0492066800021314,"d":"3.05"},{"v":1.4439905199999998,"d":"1.44"}]
["21161","Mason","KY",{"v":0.44053002399999996,"d":"0.44"},{"v":2.856658394297099,"d":"2.86"},{"v":2.8566583942970984,"d":"2.86"},{"v":1.0931412285000002,"d":"1.09"}]
["21163","Meade","KY",{"v":0.48335232200000006,"d":"0.48"},{"v":2.9446523118634924,"d":"2.94"},{"v":2.9446523118634924,"d":"2.94"},{"v":1.1985475685000002,"d":"1.20"}]
["21165","Menifee","KY",{"v":0.45901044699999993,"d":"0.46"},{"v":3.060773715930261,"d":"3.06"},{"v":3.06077371593026,"d":"3.06"},{"v":1.4940338815,"d":"1.49"}]
["21167","Mercer","KY",{"v":0.4645294099999999,"d":"0.46"},{"v":2.8409103413659484,"d":"2.84"},{"v":2.8409103413659484,"d":"2.84"},{"v":1.053031225,"d":"1.05"}]
["21169","Metcalfe","KY",{"v":0.5010174,"d":"0.50"},{"v":2.899566031983313,"d":"2.90"},{"v":2.8995660319833134,"d":"2.90"},{"v":1.237243057,"d":"1.24"}]
["21171","Monroe","KY",{"v":0.49428551299999995,"d":"0.49"},{"v":2.8864239940634215,"d":"2.89"},{"v":2.8864239940634215,"d":"2.89"},{"v":1.2465123430000002,"d":"1.25"}]
["21173","Montgomery","KY",{"v":0.44103123800000005,"d":"0.44"},{"v":2.838957776401068,"d":"2.84"},{"v":2.838957776401068,"d":"2.84"},{"v":1.0780749825,"d":"1.08"}]
["21175","Morgan","KY",{"v":0.44591057500000003,"d":"0.45"},{"v":3.156816003620034,"d":"3.16"},{"v":3.1568160036200346,"d":"3.16"},{"v":1.497321835,"d":"1.50"}]
["21177","Muhlenberg","KY",{"v":0.446803355,"d":"0.45"},{"v":2.8689354832129172,"d":"2.87"},{"v":2.8689354832129172,"d":"2.87"},{"v":1.1863848899999998,"d":"1.19"}]
["21179","Nelson","KY",{"v":0.442836563,"d":"0.44"},{"v":2.898822632083734,"d":"2.90"},{"v":2.898822632083734,"d":"2.90"},{"v":1.1343404044999998,"d":"1.13"}]
["21181","Nicholas","KY",{"v":0.516107911,"d":"0.52"},{"v":2.998441324787771,"d":"3.00"},{"v":2.998441324787771,"d":"3.00"},{"v":1.193799965,"d":"1.19"}]
["21183","Ohio","KY",{"v":0.455512805,"d":"0.46"},{"v":2.922282600342619,"d":"2.92"},{"v":2.92228260034262,"d":"2.92"},{"v":1.2153669504999998,"d":"1.22"}]
["21185","Oldham","KY",{"v":0.380886705,"d":"0.38"},{"v":2.7760779509411435,"d":"2.78"},{"v":2.776077950941143,"d":"2.78"},{"v":0.9920695390000001,"d":"0.99"}]
["21187","Owen","KY",{"v":0.483606019,"d":"0.48"},{"v":3.072820326866314,"d":"3.07"},{"v":3.072820326866314,"d":"3.07"},{"v":1.288996275,"d":"1.29"}]
["21189","Owsley","KY",{"v":0.44752264100000005,"d":"0.45"},{"v":3.1251262725399633,"d":"3.13"},{"v":3.1251262725399633,"d":"3.13"},{"v":1.544918372,"d":"1.54"}]
["21191","Pendleton","KY",{"v":0.487291979,"d":"0.49"},{"v":3.004298305519609,"d":"3.00"},{"v":3.004298305519609,"d":"3.00"},{"v":1.2744630185,"d":"1.27"}]
["21193","Perry","KY",{"v":0.41196635600000003,"d":"0.41"},{"v":3.0666923796622205,"d":"3.07"},{"v":3.0666923796622205,"d":"3.07"},{"v":1.4510701204999998,"d":"1.45"}]
["21195","Pike","KY",{"v":0.428750786,"d":"0.43"},{"v":3.0979862412641492,"d":"3.10"},{"v":3.0979862412641492,"d":"3.10"},{"v":1.45662688,"d":"1.46"}]
["21197","Powell","KY",{"v":0.41015352900000007,"d":"0.41"},{"v":2.922287810731387,"d":"2.92"},{"v":2.922287810731387,"d":"2.92"},{"v":1.4245449099999998,"d":"1.42"}]
["21199","Pulaski","KY",{"v":0.4267424349999999,"d":"0.43"},{"v":2.969173620296963,"d":"2.97"},{"v":2.969173620296964,"d":"2.97"},{"v":1.199953729,"d":"1.20"}]
["21201","Robertson","KY",{"v":0.479300028,"d":"0.48"},{"v":3.026086297449291,"d":"3.03"},{"v":3.0260862974492913,"d":"3.03"},{"v":1.3270142600000001,"d":"1.33"}]
["21203","Rockcastle","KY",{"v":0.443193744,"d":"0.44"},{"v":3.143251448203171,"d":"3.14"},{"v":3.1432514482031704,"d":"3.14"},{"v":1.370875642,"d":"1.37"}]
["21205","Rowan","KY",{"v":0.420969785,"d":"0.42"},{"v":2.9618712522812287,"d":"2.96"},{"v":2.961871252281229,"d":"2.96"},{"v":1.4186537779999997,"d":"1.42"}]
["21207","Russell","KY",{"v":0.4877540759999999,"d":"0.49"},{"v":3.024124727847212,"d":"3.02"},{"v":3.0241247278472114,"d":"3.02"},{"v":1.2387238775000002,"d":"1.24"}]
["21209","Scott","KY",{"v":0.4110895520000001,"d":"0.41"},{"v":2.8492610286935496,"d":"2.85"},{"v":2.84926102869355,"d":"2.85"},{"v":1.0174081035,"d":"1.02"}]
["21211","Shelby","KY",{"v":0.4526001719999999,"d":"0.45"},{"v":2.820995307495399,"d":"2.82"},{"v":2.8209953074953984,"d":"2.82"},{"v":1.0362682664999998,"d":"1.04"}]
["21213","Simpson","KY",{"v":0.466388938,"d":"0.47"},{"v":2.6618394765346673,"d":"2.66"},{"v":2.6618394765346673,"d":"2.66"},{"v":0.9616241864999998,"d":"0.96"}]
["21215","Spencer","KY",{"v":0.49600375500000005,"d":"0.50"},{"v":2.988147338904456,"d":"2.99"},{"v":2.988147338904456,"d":"2.99"},{"v":1.1927809379999998,"d":"1.19"}]
["21217","Taylor","KY",{"v":0.444086853,"d":"0.44"},{"v":2.807096174209896,"d":"2.81"},{"v":2.807096174209896,"d":"2.81"},{"v":1.1319177019999997,"d":"1.13"}]
["21219","Todd","KY",{"v":0.521578252,"d":"0.52"},{"v":2.9203037195201667,"d":"2.92"},{"v":2.9203037195201667,"d":"2.92"},{"v":1.1197223745,"d":"1.12"}]
["21221","Trigg","KY",{"v":0.46950557700000006,"d":"0.47"},{"v":2.928313089645313,"d":"2.93"},{"v":2.928313089645313,"d":"2.93"},{"v":1.222129656,"d":"1.22"}]
["21223","Trimble","KY",{"v":0.478453826,"d":"0.48"},{"v":3.0665068262275756,"d":"3.07"},{"v":3.066506826227576,"d":"3.07"},{"v":1.2540205775000002,"d":"1.25"}]
["21225","Union","KY",{"v":0.49148285599999997,"d":"0.49"},{"v":2.8232515693628275,"d":"2.82"},{"v":2.823251569362828,"d":"2.82"},{"v":1.0406409575,"d":"1.04"}]
["21227","Warren","KY",{"v":0.40595705899999995,"d":"0.41"},{"v":2.700299643693613,"d":"2.70"},{"v":2.700299643693613,"d":"2.70"},{"v":1.0107612215,"d":"1.01"}]
["21229","Washington","KY",{"v":0.50924706,"d":"0.51"},{"v":2.9148272331423772,"d":"2.91"},{"v":2.9148272331423772,"d":"2.91"},{"v":1.1929692415000002,"d":"1.19"}]
["21231","Wayne","KY",{"v":0.43317457100000006,"d":"0.43"},{"v":3.0941553802738437,"d":"3.09"},{"v":3.0941553802738446,"d":"3.09"},{"v":1.3290816269999999,"d":"1.33"}]
["21233","Webster","KY",{"v":0.51594145,"d":"0.52"},{"v":2.8733510711436634,"d":"2.87"},{"v":2.873351071143664,"d":"2.87"},{"v":1.1373445279999999,"d":"1.14"}]
["21235","Whitley","KY",{"v":0.41205074199999997,"d":"0.41"},{"v":2.9309012020025165,"d":"2.93"},{"v":2.9309012020025165,"d":"2.93"},{"v":1.3897554860000003,"d":"1.39"}]
["21237","Wolfe","KY",{"v":0.451595216,"d":"0.45"},{"v":3.1013770763003685,"d":"3.10"},{"v":3.101377076300369,"d":"3.10"},{"v":1.5026863685,"d":"1.50"}]
["21239","Woodford","KY",{"v":0.4438601119999999,"d":"0.44"},{"v":2.8162341834794358,"d":"2.82"},{"v":2.8162341834794367,"d":"2.82"},{"v":0.9615108085,"d":"0.96"}]
["22001","Acadia","LA",{"v":0.125008228,"d":"0.13"},{"v":0.6294060669204593,"d":"0.63"},{"v":0.6294060669204593,"d":"0.63"},{"v":0.2418335345,"d":"0.24"}]
["22003","Allen","LA",{"v":0.121135881,"d":"0.12"},{"v":0.6389858458965171,"d":"0.64"},{"v":0.6389858458965171,"d":"0.64"},{"v":0.333976952,"d":"0.33"}]
["22005","Ascension","LA",{"v":0.098038994,"d":"0.10"},{"v":0.6037452090547705,"d":"0.60"},{"v":0.6037452090547706,"d":"0.60"},{"v":0.24695628150000007,"d":"0.25"}]
["22007","Assumption","LA",{"v":0.115540531,"d":"0.12"},{"v":0.6397627184486075,"d":"0.64"},{"v":0.6397627184486075,"d":"0.64"},{"v":0.282777241,"d":"0.28"}]
["22009","Avoyelles","LA",{"v":0.12530028600000004,"d":"0.13"},{"v":0.6267682489432482,"d":"0.63"},{"v":0.6267682489432482,"d":"0.63"},{"v":0.279575332,"d":"0.28"}]
["22011","Beauregard","LA",{"v":0.117830832,"d":"0.12"},{"v":0.6571920142220583,"d":"0.66"},{"v":0.6571920142220583,"d":"0.66"},{"v":0.3316927975,"d":"0.33"}]
["22013","Bienville","LA",{"v":0.11885555000000002,"d":"0.12"},{"v":0.6790005375168884,"d":"0.68"},{"v":0.6790005375168884,"d":"0.68"},{"v":0.35677977450000004,"d":"0.36"}]
["22015","Bossier","LA",{"v":0.10169136999999999,"d":"0.10"},{"v":0.647501101420361,"d":"0.65"},{"v":0.647501101420361,"d":"0.65"},{"v":0.29407149850000003,"d":"0.29"}]
["22017","Caddo","LA",{"v":0.09728674300000001,"d":"0.10"},{"v":0.6316196747576875,"d":"0.63"},{"v":0.6316196747576874,"d":"0.63"},{"v":0.26583711849999997,"d":"0.27"}]
["22019","Calcasieu","LA",{"v":0.10695810799999998,"d":"0.11"},{"v":0.6175609237072092,"d":"0.62"},{"v":0.617560923707209,"d":"0.62"},{"v":0.24389332100000002,"d":"0.24"}]
["22021","Caldwell","LA",{"v":0.126127493,"d":"0.13"},{"v":0.6944142743594178,"d":"0.69"},{"v":0.6944142743594178,"d":"0.69"},{"v":0.34679964350000003,"d":"0.35"}]
["22023","Cameron","LA",{"v":0.152142371,"d":"0.15"},{"v":0.6717060197507457,"d":"0.67"},{"v":0.6717060197507457,"d":"0.67"},{"v":0.24091606349999997,"d":"0.24"}]
["22025","Catahoula","LA",{"v":0.137879566,"d":"0.14"},{"v":0.6531750747223956,"d":"0.65"},{"v":0.6531750747223956,"d":"0.65"},{"v":0.29459836549999996,"d":"0.29"}]
["22027","Claiborne","LA",{"v":0.11697447799999999,"d":"0.12"},{"v":0.6631937412618936,"d":"0.66"},{"v":0.6631937412618936,"d":"0.66"},{"v":0.3621624465000001,"d":"0.36"}]
["22029","Concordia","LA",{"v":0.11621757200000002,"d":"0.12"},{"v":0.6311932275170838,"d":"0.63"},{"v":0.6311932275170838,"d":"0.63"},{"v":0.25929641200000003,"d":"0.26"}]
["22031","De Soto","LA",{"v":0.12009112399999998,"d":"0.12"},{"v":0.6785694379929734,"d":"0.68"},{"v":0.6785694379929734,"d":"0.68"},{"v":0.3300861375,"d":"0.33"}]
["22033","East Baton Rouge","LA",{"v":0.076440736,"d":"0.08"},{"v":0.4916284172913714,"d":"0.49"},{"v":0.4916284172913714,"d":"0.49"},{"v":0.23882250650000003,"d":"0.24"}]
["22035","East Carroll","LA",{"v":0.12008894199999999,"d":"0.12"},{"v":0.601569089001128,"d":"0.60"},{"v":0.601569089001128,"d":"0.60"},{"v":0.24461069500000002,"d":"0.24"}]
["22037","East Feliciana","LA",{"v":0.127328774,"d":"0.13"},{"v":0.6627139729104732,"d":"0.66"},{"v":0.6627139729104732,"d":"0.66"},{"v":0.344602932,"d":"0.34"}]
["22039","Evangeline","LA",{"v":0.120748753,"d":"0.12"},{"v":0.6428354900469689,"d":"0.64"},{"v":0.6428354900469689,"d":"0.64"},{"v":0.2849888075,"d":"0.28"}]
["22041","Franklin","LA",{"v":0.131087259,"d":"0.13"},{"v":0.6726390592801542,"d":"0.67"},{"v":0.6726390592801541,"d":"0.67"},{"v":0.26754584400000003,"d":"0.27"}]
["22043","Grant","LA",{"v":0.126098115,"d":"0.13"},{"v":0.6814611928970211,"d":"0.68"},{"v":0.6814611928970211,"d":"0.68"},{"v":0.34904126950000003,"d":"0.35"}]
["22045","Iberia","LA",{"v":0.11729770000000002,"d":"0.12"},{"v":0.6201336551362209,"d":"0.62"},{"v":0.6201336551362209,"d":"0.62"},{"v":0.22561722249999994,"d":"0.23"}]
["22047","Iberville","LA",{"v":0.11679931200000002,"d":"0.12"},{"v":0.6171802280422192,"d":"0.62"},{"v":0.6171802280422192,"d":"0.62"},{"v":0.3156082734999999,"d":"0.32"}]
["22049","Jackson","LA",{"v":0.11496213299999998,"d":"0.11"},{"v":0.6625402858179249,"d":"0.66"},{"v":0.6625402858179249,"d":"0.66"},{"v":0.35669188399999996,"d":"0.36"}]
["22051","Jefferson","LA",{"v":0.073942339,"d":"0.07"},{"v":0.1946764959789789,"d":"0.19"},{"v":0.1946764959789789,"d":"0.19"},{"v":0.16838482150000003,"d":"0.17"}]
["22053","Jefferson Davis","LA",{"v":0.128284815,"d":"0.13"},{"v":0.6273591601061852,"d":"0.63"},{"v":0.6273591601061852,"d":"0.63"},{"v":0.24077800049999998,"d":"0.24"}]
["22055","Lafayette","LA",{"v":0.08727320899999999,"d":"0.09"},{"v":0.5331352192791262,"d":"0.53"},{"v":0.5331352192791261,"d":"0.53"},{"v":0.19700059300000003,"d":"0.20"}]
["22057","Lafourche","LA",{"v":0.12112372400000002,"d":"0.12"},{"v":0.6140162148849901,"d":"0.61"},{"v":0.6140162148849901,"d":"0.61"},{"v":0.21679244849999998,"d":"0.22"}]
["22059","LaSalle","LA",{"v":0.118583633,"d":"0.12"},{"v":0.6565285556018742,"d":"0.66"},{"v":0.6565285556018742,"d":"0.66"},{"v":0.3476367390000001,"d":"0.35"}]
["22061","Lincoln","LA",{"v":0.103189483,"d":"0.10"},{"v":0.6096475243433567,"d":"0.61"},{"v":0.6096475243433566,"d":"0.61"},{"v":0.3339119910000001,"d":"0.33"}]
["22063","Livingston","LA",{"v":0.10419381,"d":"0.10"},{"v":0.6500067453390498,"d":"0.65"},{"v":0.6500067453390499,"d":"0.65"},{"v":0.30878051,"d":"0.31"}]
["22065","Madison","LA",{"v":0.11594884,"d":"0.12"},{"v":0.6288259445874326,"d":"0.63"},{"v":0.6288259445874327,"d":"0.63"},{"v":0.252832505,"d":"0.25"}]
["22067","Morehouse","LA",{"v":0.12049984799999999,"d":"0.12"},{"v":0.6638114129536954,"d":"0.66"},{"v":0.6638114129536954,"d":"0.66"},{"v":0.2762254,"d":"0.28"}]
["22069","Natchitoches","LA",{"v":0.11380972,"d":"0.11"},{"v":0.6744435693131091,"d":"0.67"},{"v":0.6744435693131091,"d":"0.67"},{"v":0.313687521,"d":"0.31"}]
["22071","Orleans","LA",{"v":0.058672379999999996,"d":"0.06"},{"v":0.008492271253232502,"d":"0.01"},{"v":0.008492271253232504,"d":"0.01"},{"v":0.16033538750000004,"d":"0.16"}]
["22073","Ouachita","LA",{"v":0.100484131,"d":"0.10"},{"v":0.6446835069137408,"d":"0.64"},{"v":0.6446835069137408,"d":"0.64"},{"v":0.285645136,"d":"0.29"}]
["22075","Plaquemines","LA",{"v":0.128658082,"d":"0.13"},{"v":0.6245585224005825,"d":"0.62"},{"v":0.6245585224005825,"d":"0.62"},{"v":0.201314585,"d":"0.20"}]
["22077","Pointe Coupee","LA",{"v":0.12270567300000002,"d":"0.12"},{"v":0.6250023671138794,"d":"0.63"},{"v":0.6250023671138792,"d":"0.63"},{"v":0.280037237,"d":"0.28"}]
["22079","Rapides","LA",{"v":0.108501243,"d":"0.11"},{"v":0.6322738542820343,"d":"0.63"},{"v":0.6322738542820343,"d":"0.63"},{"v":0.3068558854999999,"d":"0.31"}]
["22081","Red River","LA",{"v":0.131248613,"d":"0.13"},{"v":0.6644572450775753,"d":"0.66"},{"v":0.6644572450775752,"d":"0.66"},{"v":0.318803014,"d":"0.32"}]
["22083","Richland","LA",{"v":0.12763421499999997,"d":"0.13"},{"v":0.6550426826101765,"d":"0.66"},{"v":0.6550426826101765,"d":"0.66"},{"v":0.26715852100000004,"d":"0.27"}]
["22085","Sabine","LA",{"v":0.12337150600000002,"d":"0.12"},{"v":0.6937257530197143,"d":"0.69"},{"v":0.6937257530197145,"d":"0.69"},{"v":0.33311036149999995,"d":"0.33"}]
["22087","St Bernard","LA",{"v":0.12013983700000001,"d":"0.12"},{"v":0.5677194475397267,"d":"0.57"},{"v":0.5677194475397268,"d":"0.57"},{"v":0.18954805799999996,"d":"0.19"}]
["22089","St Charles","LA",{"v":0.11282973,"d":"0.11"},{"v":0.5970981037543741,"d":"0.60"},{"v":0.5970981037543742,"d":"0.60"},{"v":0.21214675500000002,"d":"0.21"}]
["22091","St Helena","LA",{"v":0.126328859,"d":"0.13"},{"v":0.6980964408627724,"d":"0.70"},{"v":0.6980964408627726,"d":"0.70"},{"v":0.34852852700000003,"d":"0.35"}]
["22093","St James","LA",{"v":0.11250474,"d":"0.11"},{"v":0.5989957933997124,"d":"0.60"},{"v":0.5989957933997124,"d":"0.60"},{"v":0.275307911,"d":"0.28"}]
["22095","St John The Baptist","LA",{"v":0.11001819500000001,"d":"0.11"},{"v":0.6158830548772257,"d":"0.62"},{"v":0.6158830548772258,"d":"0.62"},{"v":0.2306842845,"d":"0.23"}]
["22097","St Landry","LA",{"v":0.118305562,"d":"0.12"},{"v":0.6323773523994083,"d":"0.63"},{"v":0.6323773523994083,"d":"0.63"},{"v":0.2665321495,"d":"0.27"}]
["22099","St Martin","LA",{"v":0.114991917,"d":"0.11"},{"v":0.6543550948870713,"d":"0.65"},{"v":0.6543550948870713,"d":"0.65"},{"v":0.296675305,"d":"0.30"}]
["22101","St Mary","LA",{"v":0.110909023,"d":"0.11"},{"v":0.6251005665830948,"d":"0.63"},{"v":0.6251005665830947,"d":"0.63"},{"v":0.2313664635,"d":"0.23"}]
["22103","St Tammany","LA",{"v":0.10149369499999998,"d":"0.10"},{"v":0.618128633429607,"d":"0.62"},{"v":0.6181286334296071,"d":"0.62"},{"v":0.2712701025,"d":"0.27"}]
["22105","Tangipahoa","LA",{"v":0.11108730499999998,"d":"0.11"},{"v":0.6312217522193232,"d":"0.63"},{"v":0.6312217522193232,"d":"0.63"},{"v":0.28537054450000005,"d":"0.29"}]
["22107","Tensas","LA",{"v":0.140507218,"d":"0.14"},{"v":0.6513820898303526,"d":"0.65"},{"v":0.6513820898303526,"d":"0.65"},{"v":0.286934723,"d":"0.29"}]
["22109","Terrebonne","LA",{"v":0.12029259899999999,"d":"0.12"},{"v":0.6103104626622177,"d":"0.61"},{"v":0.6103104626622178,"d":"0.61"},{"v":0.206172641,"d":"0.21"}]
["22111","Union","LA",{"v":0.118646072,"d":"0.12"},{"v":0.6918946435042926,"d":"0.69"},{"v":0.6918946435042925,"d":"0.69"},{"v":0.3527911165,"d":"0.35"}]
["22113","Vermilion","LA",{"v":0.132879405,"d":"0.13"},{"v":0.6415021383731124,"d":"0.64"},{"v":0.6415021383731123,"d":"0.64"},{"v":0.22558602799999997,"d":"0.23"}]
["22115","Vernon","LA",{"v":0.118499423,"d":"0.12"},{"v":0.6674223596259466,"d":"0.67"},{"v":0.6674223596259465,"d":"0.67"},{"v":0.33542508349999994,"d":"0.34"}]
["22117","Washington","LA",{"v":0.117184912,"d":"0.12"},{"v":0.6470205819182666,"d":"0.65"},{"v":0.6470205819182666,"d":"0.65"},{"v":0.31886415999999995,"d":"0.32"}]
["22119","Webster","LA",{"v":0.11018344699999999,"d":"0.11"},{"v":0.6433376182489111,"d":"0.64"},{"v":0.643337618248911,"d":"0.64"},{"v":0.3331754445,"d":"0.33"}]
["22121","West Baton Rouge","LA",{"v":0.10989619399999999,"d":"0.11"},{"v":0.6288074846588804,"d":"0.63"},{"v":0.6288074846588804,"d":"0.63"},{"v":0.268241753,"d":"0.27"}]
["22123","West Carroll","LA",{"v":0.143186534,"d":"0.14"},{"v":0.6716762065221203,"d":"0.67"},{"v":0.6716762065221202,"d":"0.67"},{"v":0.26744853900000004,"d":"0.27"}]
["22125","West Feliciana","LA",{"v":0.130459675,"d":"0.13"},{"v":0.655653114646783,"d":"0.66"},{"v":0.655653114646783,"d":"0.66"},{"v":0.33710432500000004,"d":"0.34"}]
["22127","Winn","LA",{"v":0.112189317,"d":"0.11"},{"v":0.6854878126013161,"d":"0.69"},{"v":0.6854878126013161,"d":"0.69"},{"v":0.362583737,"d":"0.36"}]
["23001","Androscoggin","ME",{"v":0.44064245299999993,"d":"0.44"},{"v":4.237498996286706,"d":"4.24"},{"v":4.237498996286706,"d":"4.24"},{"v":1.7055194969999998,"d":"1.71"}]
["23003","Aroostook","ME",{"v":0.504034063,"d":"0.50"},{"v":4.862846261431427,"d":"4.86"},{"v":4.862846261431427,"d":"4.86"},{"v":1.977571982,"d":"1.98"}]
["23005","Cumberland","ME",{"v":0.454266693,"d":"0.45"},{"v":4.0665399045205906,"d":"4.07"},{"v":4.0665399045205906,"d":"4.07"},{"v":1.4714415425,"d":"1.47"}]
["23007","Franklin","ME",{"v":0.5056692760000001,"d":"0.51"},{"v":4.948538497438645,"d":"4.95"},{"v":4.948538497438646,"d":"4.95"},{"v":2.074348582,"d":"2.07"}]
["23009","Hancock","ME",{"v":0.5735409630000001,"d":"0.57"},{"v":4.31997691625766,"d":"4.32"},{"v":4.319976916257659,"d":"4.32"},{"v":1.6742634880000002,"d":"1.67"}]
["23011","Kennebec","ME",{"v":0.48569849,"d":"0.49"},{"v":4.399318542780461,"d":"4.40"},{"v":4.399318542780461,"d":"4.40"},{"v":1.7487785015000004,"d":"1.75"}]
["23013","Knox","ME",{"v":0.5579517260000001,"d":"0.56"},{"v":4.165018879555586,"d":"4.17"},{"v":4.165018879555586,"d":"4.17"},{"v":1.4113083020000001,"d":"1.41"}]
["23015","Lincoln","ME",{"v":0.589746336,"d":"0.59"},{"v":4.328295042339517,"d":"4.33"},{"v":4.328295042339517,"d":"4.33"},{"v":1.6440389894999996,"d":"1.64"}]
["23017","Oxford","ME",{"v":0.49149615499999993,"d":"0.49"},{"v":4.937757286829759,"d":"4.94"},{"v":4.937757286829759,"d":"4.94"},{"v":2.054052825,"d":"2.05"}]
["23019","Penobscot","ME",{"v":0.49350468999999997,"d":"0.49"},{"v":4.456958400273487,"d":"4.46"},{"v":4.456958400273487,"d":"4.46"},{"v":1.8217926639999995,"d":"1.82"}]
["23021","Piscataquis","ME",{"v":0.5392926450000001,"d":"0.54"},{"v":4.920890165451439,"d":"4.92"},{"v":4.920890165451439,"d":"4.92"},{"v":2.0177037245,"d":"2.02"}]
["23023","Sagadahoc","ME",{"v":0.519512256,"d":"0.52"},{"v":4.194044972617777,"d":"4.19"},{"v":4.194044972617778,"d":"4.19"},{"v":1.5562345515,"d":"1.56"}]
["23025","Somerset","ME",{"v":0.50422842,"d":"0.50"},{"v":4.91195070105266,"d":"4.91"},{"v":4.91195070105266,"d":"4.91"},{"v":2.0036600035000003,"d":"2.00"}]
["23027","Waldo","ME",{"v":0.5471649119999998,"d":"0.55"},{"v":4.420037555010597,"d":"4.42"},{"v":4.420037555010598,"d":"4.42"},{"v":1.8066437694999997,"d":"1.81"}]
["23029","Washington","ME",{"v":0.5593970100000001,"d":"0.56"},{"v":4.519968004749255,"d":"4.52"},{"v":4.519968004749255,"d":"4.52"},{"v":1.781045174,"d":"1.78"}]
["23031","York","ME",{"v":0.49003900799999994,"d":"0.49"},{"v":4.222787278512288,"d":"4.22"},{"v":4.222787278512288,"d":"4.22"},{"v":1.628218524,"d":"1.63"}]
["24001","Allegany","MD",{"v":0.37544932400000003,"d":"0.38"},{"v":2.960750593058067,"d":"2.96"},{"v":2.960750593058067,"d":"2.96"},{"v":1.3685367265000001,"d":"1.37"}]
["24003","Anne Arundel","MD",{"v":0.281622631,"d":"0.28"},{"v":1.488539645811621,"d":"1.49"},{"v":1.488539645811621,"d":"1.49"},{"v":0.8861515904999999,"d":"0.89"}]
["24005","Baltimore","MD",{"v":0.279974777,"d":"0.28"},{"v":1.319530098868768,"d":"1.32"},{"v":1.3195300988687682,"d":"1.32"},{"v":0.8829696464999999,"d":"0.88"}]
["24009","Calvert","MD",{"v":0.4088266420000001,"d":"0.41"},{"v":2.882783579355138,"d":"2.88"},{"v":2.882783579355138,"d":"2.88"},{"v":0.9935922320000001,"d":"0.99"}]
["24011","Caroline","MD",{"v":0.495649059,"d":"0.50"},{"v":2.9534824446469297,"d":"2.95"},{"v":2.95348244464693,"d":"2.95"},{"v":1.1071511765,"d":"1.11"}]
["24013","Carroll","MD",{"v":0.415603655,"d":"0.42"},{"v":2.95667831279625,"d":"2.96"},{"v":2.95667831279625,"d":"2.96"},{"v":1.022540468,"d":"1.02"}]
["24015","Cecil","MD",{"v":0.417518526,"d":"0.42"},{"v":2.9742313786684518,"d":"2.97"},{"v":2.9742313786684518,"d":"2.97"},{"v":1.042311505,"d":"1.04"}]
["24017","Charles","MD",{"v":0.41440840700000003,"d":"0.41"},{"v":2.957172985440937,"d":"2.96"},{"v":2.9571729854409368,"d":"2.96"},{"v":1.101434938,"d":"1.10"}]
["24019","Dorchester","MD",{"v":0.487042817,"d":"0.49"},{"v":2.8836743994465612,"d":"2.88"},{"v":2.8836743994465612,"d":"2.88"},{"v":1.0079007024999997,"d":"1.01"}]
["24021","Frederick","MD",{"v":0.407848607,"d":"0.41"},{"v":2.996075546187924,"d":"3.00"},{"v":2.996075546187924,"d":"3.00"},{"v":1.019495954,"d":"1.02"}]
["24023","Garrett","MD",{"v":0.440480839,"d":"0.44"},{"v":3.381862103242798,"d":"3.38"},{"v":3.381862103242798,"d":"3.38"},{"v":1.4635548714999997,"d":"1.46"}]
["24025","Harford","MD",{"v":0.381016977,"d":"0.38"},{"v":2.874022495249372,"d":"2.87"},{"v":2.8740224952493723,"d":"2.87"},{"v":0.9543534815,"d":"0.95"}]
["24027","Howard","MD",{"v":0.291252743,"d":"0.29"},{"v":1.9269935375611358,"d":"1.93"},{"v":1.9269935375611356,"d":"1.93"},{"v":0.9251451004999999,"d":"0.93"}]
["24029","Kent","MD",{"v":0.506854163,"d":"0.51"},{"v":2.9900861700769683,"d":"2.99"},{"v":2.990086170076968,"d":"2.99"},{"v":1.0319823125,"d":"1.03"}]
["24031","Montgomery","MD",{"v":0.20572310799999996,"d":"0.21"},{"v":0.21745410257437292,"d":"0.22"},{"v":0.21745410257437292,"d":"0.22"},{"v":0.846840175,"d":"0.85"}]
["24033","Prince Georges","MD",{"v":0.21839801100000003,"d":"0.22"},{"v":0.5816307629920698,"d":"0.58"},{"v":0.58163076299207,"d":"0.58"},{"v":0.8951420259999999,"d":"0.90"}]
["24035","Queen Annes","MD",{"v":0.47738115000000003,"d":"0.48"},{"v":2.9895703626151304,"d":"2.99"},{"v":2.98957036261513,"d":"2.99"},{"v":1.0113494705,"d":"1.01"}]
["24037","St Marys","MD",{"v":0.431431364,"d":"0.43"},{"v":2.91216854347629,"d":"2.91"},{"v":2.91216854347629,"d":"2.91"},{"v":1.0435449465000002,"d":"1.04"}]
["24039","Somerset","MD",{"v":0.47916229799999993,"d":"0.48"},{"v":2.89355707101972,"d":"2.89"},{"v":2.8935570710197194,"d":"2.89"},{"v":1.0128513785,"d":"1.01"}]
["24041","Talbot","MD",{"v":0.485588185,"d":"0.49"},{"v":2.8577263183061175,"d":"2.86"},{"v":2.8577263183061175,"d":"2.86"},{"v":0.9809721909999999,"d":"0.98"}]
["24043","Washington","MD",{"v":0.40083145200000003,"d":"0.40"},{"v":3.0699095006158825,"d":"3.07"},{"v":3.0699095006158825,"d":"3.07"},{"v":1.0941281189999998,"d":"1.09"}]
["24045","Wicomico","MD",{"v":0.39544875999999995,"d":"0.40"},{"v":2.828205436612643,"d":"2.83"},{"v":2.8282054366126435,"d":"2.83"},{"v":1.0311813630000002,"d":"1.03"}]
["24047","Worcester","MD",{"v":0.39035731600000007,"d":"0.39"},{"v":2.920722197544037,"d":"2.92"},{"v":2.9207221975440376,"d":"2.92"},{"v":1.0202315849999997,"d":"1.02"}]
["24510","Baltimore City","MD",{"v":0.047493244000000004,"d":"0.05"},{"v":4.4837134641583375E-11,"d":"0.00"},{"v":4.483713464158338e-11,"d":"0.00"},{"v":0.561855955,"d":"0.56"}]
["25001","Barnstable","MA",{"v":0.270935066,"d":"0.27"},{"v":2.0260506280827713,"d":"2.03"},{"v":2.0260506280827713,"d":"2.03"},{"v":0.6509337765000002,"d":"0.65"}]
["25003","Berkshire","MA",{"v":0.269871019,"d":"0.27"},{"v":2.395408344434613,"d":"2.40"},{"v":2.395408344434613,"d":"2.40"},{"v":1.0900376585,"d":"1.09"}]
["25005","Bristol","MA",{"v":0.217701392,"d":"0.22"},{"v":1.5725396250887245,"d":"1.57"},{"v":1.5725396250887247,"d":"1.57"},{"v":0.7807582135,"d":"0.78"}]
["25007","Dukes","MA",{"v":0.337447747,"d":"0.34"},{"v":2.289409757202505,"d":"2.29"},{"v":2.289409757202505,"d":"2.29"},{"v":0.7130102819999999,"d":"0.71"}]
["25009","Essex","MA",{"v":0.183451416,"d":"0.18"},{"v":0.5880729043929942,"d":"0.59"},{"v":0.5880729043929942,"d":"0.59"},{"v":0.6623920754999999,"d":"0.66"}]
["25011","Franklin","MA",{"v":0.293309773,"d":"0.29"},{"v":2.3774322803948533,"d":"2.38"},{"v":2.3774322803948538,"d":"2.38"},{"v":1.118400445,"d":"1.12"}]
["25013","Hampden","MA",{"v":0.212681365,"d":"0.21"},{"v":1.9408680249779968,"d":"1.94"},{"v":1.9408680249779968,"d":"1.94"},{"v":0.9037111019999999,"d":"0.90"}]
["25015","Hampshire","MA",{"v":0.25930425,"d":"0.26"},{"v":2.2920425685956167,"d":"2.29"},{"v":2.292042568595617,"d":"2.29"},{"v":1.0136485530000001,"d":"1.01"}]
["25017","Middlesex","MA",{"v":0.14755946799999997,"d":"0.15"},{"v":0.19885392552895778,"d":"0.20"},{"v":0.19885392552895778,"d":"0.20"},{"v":0.755105781,"d":"0.76"}]
["25019","Nantucket","MA",{"v":0.319603223,"d":"0.32"},{"v":2.2257988260546386,"d":"2.23"},{"v":2.2257988260546386,"d":"2.23"},{"v":0.6593458445,"d":"0.66"}]
["25021","Norfolk","MA",{"v":0.156000145,"d":"0.16"},{"v":0.36488178650419784,"d":"0.36"},{"v":0.3648817865041978,"d":"0.36"},{"v":0.7298881905000001,"d":"0.73"}]
["25023","Plymouth","MA",{"v":0.239851779,"d":"0.24"},{"v":1.990775556680413,"d":"1.99"},{"v":1.9907755566804128,"d":"1.99"},{"v":0.719130374,"d":"0.72"}]
["25025","Suffolk","MA",{"v":0.004233319,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.29465231999999997,"d":"0.29"}]
["25027","Worcester","MA",{"v":0.244703766,"d":"0.24"},{"v":2.216229260076873,"d":"2.22"},{"v":2.216229260076873,"d":"2.22"},{"v":0.9291298880000003,"d":"0.93"}]
["26001","Alcona","MI",{"v":0.289169872,"d":"0.29"},{"v":2.2733255323405848,"d":"2.27"},{"v":2.2733255323405848,"d":"2.27"},{"v":0.9318922709999998,"d":"0.93"}]
["26003","Alger","MI",{"v":0.265174431,"d":"0.27"},{"v":2.3434976992030774,"d":"2.34"},{"v":2.343497699203077,"d":"2.34"},{"v":0.9507571904999997,"d":"0.95"}]
["26005","Allegan","MI",{"v":0.282508085,"d":"0.28"},{"v":1.982552213066372,"d":"1.98"},{"v":1.9825522130663717,"d":"1.98"},{"v":0.724118432,"d":"0.72"}]
["26007","Alpena","MI",{"v":0.26329265700000004,"d":"0.26"},{"v":2.1126113006154457,"d":"2.11"},{"v":2.1126113006154457,"d":"2.11"},{"v":0.7879145729999998,"d":"0.79"}]
["26009","Antrim","MI",{"v":0.29871795000000007,"d":"0.30"},{"v":2.197568590037485,"d":"2.20"},{"v":2.197568590037485,"d":"2.20"},{"v":0.8594089205,"d":"0.86"}]
["26011","Arenac","MI",{"v":0.313840494,"d":"0.31"},{"v":2.102727956969652,"d":"2.10"},{"v":2.1027279569696526,"d":"2.10"},{"v":0.786199005,"d":"0.79"}]
["26013","Baraga","MI",{"v":0.276811316,"d":"0.28"},{"v":2.3822648724169873,"d":"2.38"},{"v":2.3822648724169873,"d":"2.38"},{"v":1.0035255175000002,"d":"1.00"}]
["26015","Barry","MI",{"v":0.289963769,"d":"0.29"},{"v":2.03283876373242,"d":"2.03"},{"v":2.0328387637324195,"d":"2.03"},{"v":0.7662393034999999,"d":"0.77"}]
["26017","Bay","MI",{"v":0.254093364,"d":"0.25"},{"v":1.928925463828947,"d":"1.93"},{"v":1.9289254638289473,"d":"1.93"},{"v":0.641125735,"d":"0.64"}]
["26019","Benzie","MI",{"v":0.30184955300000005,"d":"0.30"},{"v":2.1755804054846495,"d":"2.18"},{"v":2.1755804054846495,"d":"2.18"},{"v":0.848378953,"d":"0.85"}]
["26021","Berrien","MI",{"v":0.251005051,"d":"0.25"},{"v":1.9024907219112526,"d":"1.90"},{"v":1.9024907219112523,"d":"1.90"},{"v":0.6555600665000001,"d":"0.66"}]
["26023","Branch","MI",{"v":0.290560333,"d":"0.29"},{"v":2.002241491146259,"d":"2.00"},{"v":2.0022414911462594,"d":"2.00"},{"v":0.7105025315000001,"d":"0.71"}]
["26025","Calhoun","MI",{"v":0.24673919199999997,"d":"0.25"},{"v":1.9091652723771484,"d":"1.91"},{"v":1.9091652723771484,"d":"1.91"},{"v":0.6761616885,"d":"0.68"}]
["26027","Cass","MI",{"v":0.29103255799999994,"d":"0.29"},{"v":2.0075653917852194,"d":"2.01"},{"v":2.0075653917852194,"d":"2.01"},{"v":0.7328657635000001,"d":"0.73"}]
["26029","Charlevoix","MI",{"v":0.284793276,"d":"0.28"},{"v":2.1191698916988835,"d":"2.12"},{"v":2.1191698916988835,"d":"2.12"},{"v":0.7554303689999999,"d":"0.76"}]
["26031","Cheboygan","MI",{"v":0.278617873,"d":"0.28"},{"v":2.1742626565075964,"d":"2.17"},{"v":2.174262656507596,"d":"2.17"},{"v":0.888424294,"d":"0.89"}]
["26033","Chippewa","MI",{"v":0.26055058300000006,"d":"0.26"},{"v":2.2965937214193946,"d":"2.30"},{"v":2.296593721419395,"d":"2.30"},{"v":0.8404901800000001,"d":"0.84"}]
["26035","Clare","MI",{"v":0.2701746830000001,"d":"0.27"},{"v":2.1756189643866537,"d":"2.18"},{"v":2.1756189643866537,"d":"2.18"},{"v":0.8633198149999998,"d":"0.86"}]
["26037","Clinton","MI",{"v":0.275964732,"d":"0.28"},{"v":1.9641897117042555,"d":"1.96"},{"v":1.9641897117042555,"d":"1.96"},{"v":0.6777524375,"d":"0.68"}]
["26039","Crawford","MI",{"v":0.268595752,"d":"0.27"},{"v":2.26825321044405,"d":"2.27"},{"v":2.26825321044405,"d":"2.27"},{"v":0.9172960064999999,"d":"0.92"}]
["26041","Delta","MI",{"v":0.24912036800000004,"d":"0.25"},{"v":2.2437069653371333,"d":"2.24"},{"v":2.2437069653371338,"d":"2.24"},{"v":0.8291736135000001,"d":"0.83"}]
["26043","Dickinson","MI",{"v":0.224388761,"d":"0.22"},{"v":2.2874250511973737,"d":"2.29"},{"v":2.287425051197374,"d":"2.29"},{"v":0.947422097,"d":"0.95"}]
["26045","Eaton","MI",{"v":0.257268619,"d":"0.26"},{"v":1.9596513416565833,"d":"1.96"},{"v":1.9596513416565828,"d":"1.96"},{"v":0.6625206495,"d":"0.66"}]
["26047","Emmet","MI",{"v":0.276056024,"d":"0.28"},{"v":2.1343308931350684,"d":"2.13"},{"v":2.1343308931350684,"d":"2.13"},{"v":0.8164184734999999,"d":"0.82"}]
["26049","Genesee","MI",{"v":0.211305862,"d":"0.21"},{"v":1.7531579319335102,"d":"1.75"},{"v":1.7531579319335102,"d":"1.75"},{"v":0.609948794,"d":"0.61"}]
["26051","Gladwin","MI",{"v":0.288388747,"d":"0.29"},{"v":2.1558199007664394,"d":"2.16"},{"v":2.1558199007664394,"d":"2.16"},{"v":0.8535884074999999,"d":"0.85"}]
["26053","Gogebic","MI",{"v":0.24593375,"d":"0.25"},{"v":2.3428521168062,"d":"2.34"},{"v":2.3428521168062,"d":"2.34"},{"v":1.0087963085000002,"d":"1.01"}]
["26055","Grand Traverse","MI",{"v":0.246695419,"d":"0.25"},{"v":2.0858107580996954,"d":"2.09"},{"v":2.0858107580996954,"d":"2.09"},{"v":0.7768724059999998,"d":"0.78"}]
["26057","Gratiot","MI",{"v":0.29137461699999995,"d":"0.29"},{"v":2.0370245515951035,"d":"2.04"},{"v":2.0370245515951035,"d":"2.04"},{"v":0.7161119195,"d":"0.72"}]
["26059","Hillsdale","MI",{"v":0.29259556099999995,"d":"0.29"},{"v":2.022905215105454,"d":"2.02"},{"v":2.022905215105454,"d":"2.02"},{"v":0.7223233645000001,"d":"0.72"}]
["26061","Houghton","MI",{"v":0.229574135,"d":"0.23"},{"v":2.314654659717843,"d":"2.31"},{"v":2.314654659717843,"d":"2.31"},{"v":0.9055464780000001,"d":"0.91"}]
["26063","Huron","MI",{"v":0.320646128,"d":"0.32"},{"v":2.022452062128656,"d":"2.02"},{"v":2.022452062128656,"d":"2.02"},{"v":0.7103650044999998,"d":"0.71"}]
["26065","Ingham","MI",{"v":0.214354804,"d":"0.21"},{"v":1.8444118117955133,"d":"1.84"},{"v":1.8444118117955135,"d":"1.84"},{"v":0.6087781075,"d":"0.61"}]
["26067","Ionia","MI",{"v":0.28455316899999994,"d":"0.28"},{"v":1.9938387625615366,"d":"1.99"},{"v":1.9938387625615366,"d":"1.99"},{"v":0.720446694,"d":"0.72"}]
["26069","Iosco","MI",{"v":0.27087201,"d":"0.27"},{"v":2.1413742486008283,"d":"2.14"},{"v":2.1413742486008283,"d":"2.14"},{"v":0.7997588244999999,"d":"0.80"}]
["26071","Iron","MI",{"v":0.25308338,"d":"0.25"},{"v":2.3607183277429242,"d":"2.36"},{"v":2.3607183277429247,"d":"2.36"},{"v":0.9981246140000001,"d":"1.00"}]
["26073","Isabella","MI",{"v":0.256246221,"d":"0.26"},{"v":2.0658348561166835,"d":"2.07"},{"v":2.0658348561166835,"d":"2.07"},{"v":0.7300024844999999,"d":"0.73"}]
["26075","Jackson","MI",{"v":0.252732842,"d":"0.25"},{"v":1.918487817190405,"d":"1.92"},{"v":1.9184878171904047,"d":"1.92"},{"v":0.7075319665,"d":"0.71"}]
["26077","Kalamazoo","MI",{"v":0.216322242,"d":"0.22"},{"v":1.851305692317202,"d":"1.85"},{"v":1.8513056923172018,"d":"1.85"},{"v":0.639349481,"d":"0.64"}]
["26079","Kalkaska","MI",{"v":0.27621088399999993,"d":"0.28"},{"v":2.2639738157992118,"d":"2.26"},{"v":2.2639738157992118,"d":"2.26"},{"v":0.9132455525,"d":"0.91"}]
["26081","Kent","MI",{"v":0.20017211,"d":"0.20"},{"v":1.7032406548992582,"d":"1.70"},{"v":1.7032406548992578,"d":"1.70"},{"v":0.6312860275000001,"d":"0.63"}]
["26083","Keweenaw","MI",{"v":0.309559907,"d":"0.31"},{"v":2.34215802105401,"d":"2.34"},{"v":2.34215802105401,"d":"2.34"},{"v":0.8130721455,"d":"0.81"}]
["26085","Lake","MI",{"v":0.286977136,"d":"0.29"},{"v":2.2861560811059123,"d":"2.29"},{"v":2.2861560811059123,"d":"2.29"},{"v":0.956892631,"d":"0.96"}]
["26087","Lapeer","MI",{"v":0.291476129,"d":"0.29"},{"v":1.9785439657914277,"d":"1.98"},{"v":1.9785439657914279,"d":"1.98"},{"v":0.7418504545000001,"d":"0.74"}]
["26089","Leelanau","MI",{"v":0.316077157,"d":"0.32"},{"v":2.1345636611107413,"d":"2.13"},{"v":2.1345636611107413,"d":"2.13"},{"v":0.7480641659999999,"d":"0.75"}]
["26091","Lenawee","MI",{"v":0.28406785800000006,"d":"0.28"},{"v":1.9094247876693502,"d":"1.91"},{"v":1.9094247876693502,"d":"1.91"},{"v":0.6708000960000001,"d":"0.67"}]
["26093","Livingston","MI",{"v":0.24552459200000004,"d":"0.25"},{"v":1.9106871033579558,"d":"1.91"},{"v":1.9106871033579553,"d":"1.91"},{"v":0.6902900605000001,"d":"0.69"}]
["26095","Luce","MI",{"v":0.25435488199999995,"d":"0.25"},{"v":2.325480174079209,"d":"2.33"},{"v":2.325480174079209,"d":"2.33"},{"v":0.9287216884999999,"d":"0.93"}]
["26097","Mackinac","MI",{"v":0.276604497,"d":"0.28"},{"v":2.331399946458587,"d":"2.33"},{"v":2.3313999464585864,"d":"2.33"},{"v":0.8539650585,"d":"0.85"}]
["26099","Macomb","MI",{"v":0.148881576,"d":"0.15"},{"v":0.19935521659353989,"d":"0.20"},{"v":0.19935521659353989,"d":"0.20"},{"v":0.4886700615,"d":"0.49"}]
["26101","Manistee","MI",{"v":0.268730286,"d":"0.27"},{"v":2.1405717694636195,"d":"2.14"},{"v":2.1405717694636195,"d":"2.14"},{"v":0.841646091,"d":"0.84"}]
["26103","Marquette","MI",{"v":0.235297228,"d":"0.24"},{"v":2.273547772639886,"d":"2.27"},{"v":2.2735477726398865,"d":"2.27"},{"v":0.9083089335,"d":"0.91"}]
["26105","Mason","MI",{"v":0.276649726,"d":"0.28"},{"v":2.0898119706788556,"d":"2.09"},{"v":2.0898119706788556,"d":"2.09"},{"v":0.775831043,"d":"0.78"}]
["26107","Mecosta","MI",{"v":0.274684977,"d":"0.27"},{"v":2.1126714443013612,"d":"2.11"},{"v":2.1126714443013617,"d":"2.11"},{"v":0.8176844169999998,"d":"0.82"}]
["26109","Menominee","MI",{"v":0.24933543200000002,"d":"0.25"},{"v":2.3575307456625914,"d":"2.36"},{"v":2.3575307456625914,"d":"2.36"},{"v":0.9330714275000002,"d":"0.93"}]
["26111","Midland","MI",{"v":0.247284961,"d":"0.25"},{"v":2.037418247818345,"d":"2.04"},{"v":2.0374182478183456,"d":"2.04"},{"v":0.7657033179999999,"d":"0.77"}]
["26113","Missaukee","MI",{"v":0.292089085,"d":"0.29"},{"v":2.257594632860065,"d":"2.26"},{"v":2.257594632860065,"d":"2.26"},{"v":0.9116584630000001,"d":"0.91"}]
["26115","Monroe","MI",{"v":0.26038774800000003,"d":"0.26"},{"v":1.87554666292521,"d":"1.88"},{"v":1.87554666292521,"d":"1.88"},{"v":0.627343954,"d":"0.63"}]
["26117","Montcalm","MI",{"v":0.291677841,"d":"0.29"},{"v":2.0990636866359713,"d":"2.10"},{"v":2.0990636866359713,"d":"2.10"},{"v":0.78584312,"d":"0.79"}]
["26119","Montmorency","MI",{"v":0.282264736,"d":"0.28"},{"v":2.2494673653413235,"d":"2.25"},{"v":2.249467365341324,"d":"2.25"},{"v":0.9890816024999999,"d":"0.99"}]
["26121","Muskegon","MI",{"v":0.22718316700000002,"d":"0.23"},{"v":1.9411741283977078,"d":"1.94"},{"v":1.9411741283977078,"d":"1.94"},{"v":0.6923114425,"d":"0.69"}]
["26123","Newaygo","MI",{"v":0.276684155,"d":"0.28"},{"v":2.1991158485814237,"d":"2.20"},{"v":2.1991158485814237,"d":"2.20"},{"v":0.879299116,"d":"0.88"}]
["26125","Oakland","MI",{"v":0.15687075800000003,"d":"0.16"},{"v":0.6032794219738116,"d":"0.60"},{"v":0.6032794219738116,"d":"0.60"},{"v":0.568735883,"d":"0.57"}]
["26127","Oceana","MI",{"v":0.296921127,"d":"0.30"},{"v":2.155782503175395,"d":"2.16"},{"v":2.1557825031753945,"d":"2.16"},{"v":0.8189054009999999,"d":"0.82"}]
["26129","Ogemaw","MI",{"v":0.288740054,"d":"0.29"},{"v":2.2637755219455764,"d":"2.26"},{"v":2.2637755219455764,"d":"2.26"},{"v":0.9218360105,"d":"0.92"}]
["26131","Ontonagon","MI",{"v":0.276229929,"d":"0.28"},{"v":2.419426267034966,"d":"2.42"},{"v":2.419426267034966,"d":"2.42"},{"v":1.0167450255,"d":"1.02"}]
["26133","Osceola","MI",{"v":0.297850701,"d":"0.30"},{"v":2.1919207235272213,"d":"2.19"},{"v":2.1919207235272213,"d":"2.19"},{"v":0.8714925024999999,"d":"0.87"}]
["26135","Oscoda","MI",{"v":0.281857071,"d":"0.28"},{"v":2.316972080076761,"d":"2.32"},{"v":2.316972080076761,"d":"2.32"},{"v":0.9846016355000001,"d":"0.98"}]
["26137","Otsego","MI",{"v":0.260914212,"d":"0.26"},{"v":2.2096231923539666,"d":"2.21"},{"v":2.2096231923539666,"d":"2.21"},{"v":0.9018871055000001,"d":"0.90"}]
["26139","Ottawa","MI",{"v":0.230352811,"d":"0.23"},{"v":1.8378346752959953,"d":"1.84"},{"v":1.837834675295995,"d":"1.84"},{"v":0.6107292360000001,"d":"0.61"}]
["26141","Presque Isle","MI",{"v":0.284908713,"d":"0.28"},{"v":2.1880814919766793,"d":"2.19"},{"v":2.1880814919766793,"d":"2.19"},{"v":0.8395067314999999,"d":"0.84"}]
["26143","Roscommon","MI",{"v":0.262579892,"d":"0.26"},{"v":2.1529317804023513,"d":"2.15"},{"v":2.1529317804023513,"d":"2.15"},{"v":0.8892022205,"d":"0.89"}]
["26145","Saginaw","MI",{"v":0.24929205400000004,"d":"0.25"},{"v":1.933129821950947,"d":"1.93"},{"v":1.9331298219509472,"d":"1.93"},{"v":0.6619728645,"d":"0.66"}]
["26147","St Clair","MI",{"v":0.26298955,"d":"0.26"},{"v":1.8927597557862694,"d":"1.89"},{"v":1.8927597557862696,"d":"1.89"},{"v":0.6454656019999999,"d":"0.65"}]
["26149","St Joseph","MI",{"v":0.27956568,"d":"0.28"},{"v":1.963688744698112,"d":"1.96"},{"v":1.963688744698112,"d":"1.96"},{"v":0.6891809114999999,"d":"0.69"}]
["26151","Sanilac","MI",{"v":0.315794622,"d":"0.32"},{"v":2.0595818870050073,"d":"2.06"},{"v":2.0595818870050078,"d":"2.06"},{"v":0.7226127055000001,"d":"0.72"}]
["26153","Schoolcraft","MI",{"v":0.258792957,"d":"0.26"},{"v":2.3129205573126073,"d":"2.31"},{"v":2.3129205573126077,"d":"2.31"},{"v":0.8763520985,"d":"0.88"}]
["26155","Shiawassee","MI",{"v":0.280115493,"d":"0.28"},{"v":1.952917319407544,"d":"1.95"},{"v":1.952917319407544,"d":"1.95"},{"v":0.6839302049999999,"d":"0.68"}]
["26157","Tuscola","MI",{"v":0.305208917,"d":"0.31"},{"v":2.069739112476597,"d":"2.07"},{"v":2.0697391124765967,"d":"2.07"},{"v":0.7418981404999999,"d":"0.74"}]
["26159","Van Buren","MI",{"v":0.283215383,"d":"0.28"},{"v":2.001251258204333,"d":"2.00"},{"v":2.001251258204333,"d":"2.00"},{"v":0.7461083120000002,"d":"0.75"}]
["26161","Washtenaw","MI",{"v":0.213451122,"d":"0.21"},{"v":1.83514392501363,"d":"1.84"},{"v":1.83514392501363,"d":"1.84"},{"v":0.6237568155000001,"d":"0.62"}]
["26163","Wayne","MI",{"v":0.101700465,"d":"0.10"},{"v":4.454319041652768E-3,"d":"0.00"},{"v":4.454319041652768E-3,"d":"0.00"},{"v":0.44176031250000003,"d":"0.44"}]
["26165","Wexford","MI",{"v":0.258839035,"d":"0.26"},{"v":2.200209347421513,"d":"2.20"},{"v":2.200209347421513,"d":"2.20"},{"v":0.8943800489999999,"d":"0.89"}]
["27001","Aitkin","MN",{"v":0.306697491,"d":"0.31"},{"v":2.464145483444265,"d":"2.46"},{"v":2.4641454834442653,"d":"2.46"},{"v":0.898306385,"d":"0.90"}]
["27003","Anoka","MN",{"v":0.203301475,"d":"0.20"},{"v":1.9849750095941174,"d":"1.98"},{"v":1.9849750095941174,"d":"1.98"},{"v":0.629788465,"d":"0.63"}]
["27005","Becker","MN",{"v":0.28918716200000005,"d":"0.29"},{"v":2.460198600929325,"d":"2.46"},{"v":2.460198600929325,"d":"2.46"},{"v":0.8137160915,"d":"0.81"}]
["27007","Beltrami","MN",{"v":0.281566953,"d":"0.28"},{"v":2.4590088949040108,"d":"2.46"},{"v":2.4590088949040108,"d":"2.46"},{"v":0.8121303879999999,"d":"0.81"}]
["27009","Benton","MN",{"v":0.257032803,"d":"0.26"},{"v":2.232510697264922,"d":"2.23"},{"v":2.232510697264922,"d":"2.23"},{"v":0.7014456724999999,"d":"0.70"}]
["27011","Big Stone","MN",{"v":0.330976083,"d":"0.33"},{"v":2.3001106585416036,"d":"2.30"},{"v":2.3001106585416036,"d":"2.30"},{"v":0.7609790675,"d":"0.76"}]
["27013","Blue Earth","MN",{"v":0.264492321,"d":"0.26"},{"v":2.155796650108117,"d":"2.16"},{"v":2.1557966501081167,"d":"2.16"},{"v":0.6563216295000001,"d":"0.66"}]
["27015","Brown","MN",{"v":0.27876460100000006,"d":"0.28"},{"v":2.17813421079017,"d":"2.18"},{"v":2.1781342107901702,"d":"2.18"},{"v":0.6648324985,"d":"0.66"}]
["27017","Carlton","MN",{"v":0.268658011,"d":"0.27"},{"v":2.402583736375389,"d":"2.40"},{"v":2.402583736375389,"d":"2.40"},{"v":0.8494753424999999,"d":"0.85"}]
["27019","Carver","MN",{"v":0.25447972,"d":"0.25"},{"v":2.201557817246134,"d":"2.20"},{"v":2.201557817246134,"d":"2.20"},{"v":0.6405564380000001,"d":"0.64"}]
["27021","Cass","MN",{"v":0.308456488,"d":"0.31"},{"v":2.52057084409529,"d":"2.52"},{"v":2.52057084409529,"d":"2.52"},{"v":0.8836237265000001,"d":"0.88"}]
["27023","Chippewa","MN",{"v":0.288268534,"d":"0.29"},{"v":2.236507736974298,"d":"2.24"},{"v":2.236507736974298,"d":"2.24"},{"v":0.698795564,"d":"0.70"}]
["27025","Chisago","MN",{"v":0.27684793499999993,"d":"0.28"},{"v":2.302828653068318,"d":"2.30"},{"v":2.302828653068318,"d":"2.30"},{"v":0.763848521,"d":"0.76"}]
["27027","Clay","MN",{"v":0.262977993,"d":"0.26"},{"v":2.351337099632163,"d":"2.35"},{"v":2.351337099632163,"d":"2.35"},{"v":0.6762904770000001,"d":"0.68"}]
["27029","Clearwater","MN",{"v":0.305090851,"d":"0.31"},{"v":2.5048214718476176,"d":"2.50"},{"v":2.5048214718476176,"d":"2.50"},{"v":0.8726427215,"d":"0.87"}]
["27031","Cook","MN",{"v":0.299942232,"d":"0.30"},{"v":2.5987695819397127,"d":"2.60"},{"v":2.5987695819397127,"d":"2.60"},{"v":0.938533901,"d":"0.94"}]
["27033","Cottonwood","MN",{"v":0.30853738300000005,"d":"0.31"},{"v":2.218182349613266,"d":"2.22"},{"v":2.218182349613266,"d":"2.22"},{"v":0.704759786,"d":"0.70"}]
["27035","Crow Wing","MN",{"v":0.2801699710000001,"d":"0.28"},{"v":2.3381720249468914,"d":"2.34"},{"v":2.338172024946891,"d":"2.34"},{"v":0.8035017375,"d":"0.80"}]
["27037","Dakota","MN",{"v":0.21706386700000002,"d":"0.22"},{"v":1.9489159407880734,"d":"1.95"},{"v":1.9489159407880734,"d":"1.95"},{"v":0.569861313,"d":"0.57"}]
["27039","Dodge","MN",{"v":0.295899629,"d":"0.30"},{"v":2.1933550973779066,"d":"2.19"},{"v":2.1933550973779066,"d":"2.19"},{"v":0.6928533775,"d":"0.69"}]
["27041","Douglas","MN",{"v":0.283423122,"d":"0.28"},{"v":2.2951510564980757,"d":"2.30"},{"v":2.2951510564980753,"d":"2.30"},{"v":0.714412653,"d":"0.71"}]
["27043","Faribault","MN",{"v":0.316944334,"d":"0.32"},{"v":2.231654457410698,"d":"2.23"},{"v":2.2316544574106976,"d":"2.23"},{"v":0.7265623954999999,"d":"0.73"}]
["27045","Fillmore","MN",{"v":0.319832848,"d":"0.32"},{"v":2.236846562124533,"d":"2.24"},{"v":2.236846562124533,"d":"2.24"},{"v":0.797239968,"d":"0.80"}]
["27047","Freeborn","MN",{"v":0.28530797300000005,"d":"0.29"},{"v":2.171890499591477,"d":"2.17"},{"v":2.1718904995914765,"d":"2.17"},{"v":0.6795372574999998,"d":"0.68"}]
["27049","Goodhue","MN",{"v":0.283905362,"d":"0.28"},{"v":2.1961704538552262,"d":"2.20"},{"v":2.1961704538552262,"d":"2.20"},{"v":0.7102619385000001,"d":"0.71"}]
["27051","Grant","MN",{"v":0.33302856099999995,"d":"0.33"},{"v":2.325962974826308,"d":"2.33"},{"v":2.325962974826308,"d":"2.33"},{"v":0.76509385,"d":"0.77"}]
["27053","Hennepin","MN",{"v":0.119444686,"d":"0.12"},{"v":0.03750234682524327,"d":"0.04"},{"v":0.03750234682524327,"d":"0.04"},{"v":0.5148521215,"d":"0.51"}]
["27055","Houston","MN",{"v":0.281766553,"d":"0.28"},{"v":2.2605991988562426,"d":"2.26"},{"v":2.2605991988562426,"d":"2.26"},{"v":0.8070801844999999,"d":"0.81"}]
["27057","Hubbard","MN",{"v":0.2907849350000001,"d":"0.29"},{"v":2.506240898974219,"d":"2.51"},{"v":2.5062408989742195,"d":"2.51"},{"v":0.8567767265,"d":"0.86"}]
["27059","Isanti","MN",{"v":0.2839030350000001,"d":"0.28"},{"v":2.339067195171472,"d":"2.34"},{"v":2.339067195171472,"d":"2.34"},{"v":0.7723917600000001,"d":"0.77"}]
["27061","Itasca","MN",{"v":0.28515318800000006,"d":"0.29"},{"v":2.4987311174963183,"d":"2.50"},{"v":2.4987311174963183,"d":"2.50"},{"v":0.873261011,"d":"0.87"}]
["27063","Jackson","MN",{"v":0.311000677,"d":"0.31"},{"v":2.2450858871019044,"d":"2.25"},{"v":2.2450858871019044,"d":"2.25"},{"v":0.7144300610000002,"d":"0.71"}]
["27065","Kanabec","MN",{"v":0.286680869,"d":"0.29"},{"v":2.4324540479144736,"d":"2.43"},{"v":2.432454047914474,"d":"2.43"},{"v":0.858169313,"d":"0.86"}]
["27067","Kandiyohi","MN",{"v":0.285078883,"d":"0.29"},{"v":2.2438684192818714,"d":"2.24"},{"v":2.2438684192818714,"d":"2.24"},{"v":0.6933429795,"d":"0.69"}]
["27069","Kittson","MN",{"v":0.317636201,"d":"0.32"},{"v":2.4338753715879546,"d":"2.43"},{"v":2.4338753715879546,"d":"2.43"},{"v":0.8031181150000001,"d":"0.80"}]
["27071","Koochiching","MN",{"v":0.258152799,"d":"0.26"},{"v":2.487429798116771,"d":"2.49"},{"v":2.487429798116771,"d":"2.49"},{"v":0.8617585285000001,"d":"0.86"}]
["27073","Lac Qui Parle","MN",{"v":0.333948258,"d":"0.33"},{"v":2.294299439950301,"d":"2.29"},{"v":2.2942994399503016,"d":"2.29"},{"v":0.7601782909999999,"d":"0.76"}]
["27075","Lake","MN",{"v":0.27281159999999993,"d":"0.27"},{"v":2.537991473510356,"d":"2.54"},{"v":2.537991473510356,"d":"2.54"},{"v":0.9014370060000001,"d":"0.90"}]
["27077","Lake of The Woods","MN",{"v":0.304907703,"d":"0.30"},{"v":2.517560987301142,"d":"2.52"},{"v":2.517560987301142,"d":"2.52"},{"v":0.8668094494999999,"d":"0.87"}]
["27079","Le Sueur","MN",{"v":0.30287327899999994,"d":"0.30"},{"v":2.2132387880267395,"d":"2.21"},{"v":2.2132387880267395,"d":"2.21"},{"v":0.7183292835,"d":"0.72"}]
["27081","Lincoln","MN",{"v":0.336034675,"d":"0.34"},{"v":2.2748860907403476,"d":"2.27"},{"v":2.2748860907403476,"d":"2.27"},{"v":0.7511287825,"d":"0.75"}]
["27083","Lyon","MN",{"v":0.289076186,"d":"0.29"},{"v":2.2385618066338258,"d":"2.24"},{"v":2.2385618066338258,"d":"2.24"},{"v":0.686446693,"d":"0.69"}]
["27085","McLeod","MN",{"v":0.28461240300000007,"d":"0.28"},{"v":2.2353749075433282,"d":"2.24"},{"v":2.235374907543328,"d":"2.24"},{"v":0.6880998104999999,"d":"0.69"}]
["27087","Mahnomen","MN",{"v":0.312782116,"d":"0.31"},{"v":2.4596264412892173,"d":"2.46"},{"v":2.4596264412892173,"d":"2.46"},{"v":0.8387943345000001,"d":"0.84"}]
["27089","Marshall","MN",{"v":0.317870064,"d":"0.32"},{"v":2.4277980535166734,"d":"2.43"},{"v":2.427798053516673,"d":"2.43"},{"v":0.805109908,"d":"0.81"}]
["27091","Martin","MN",{"v":0.297242944,"d":"0.30"},{"v":2.18743329749611,"d":"2.19"},{"v":2.18743329749611,"d":"2.19"},{"v":0.6924435685,"d":"0.69"}]
["27093","Meeker","MN",{"v":0.300116098,"d":"0.30"},{"v":2.2766714751326367,"d":"2.28"},{"v":2.2766714751326367,"d":"2.28"},{"v":0.7286077509999999,"d":"0.73"}]
["27095","Mille Lacs","MN",{"v":0.28697184299999995,"d":"0.29"},{"v":2.386243446416286,"d":"2.39"},{"v":2.386243446416286,"d":"2.39"},{"v":0.8107138705,"d":"0.81"}]
["27097","Morrison","MN",{"v":0.296221194,"d":"0.30"},{"v":2.3287150112585433,"d":"2.33"},{"v":2.3287150112585433,"d":"2.33"},{"v":0.7849580385,"d":"0.78"}]
["27099","Mower","MN",{"v":0.279675701,"d":"0.28"},{"v":2.142146093520033,"d":"2.14"},{"v":2.142146093520033,"d":"2.14"},{"v":0.6649267465,"d":"0.66"}]
["27101","Murray","MN",{"v":0.337576549,"d":"0.34"},{"v":2.280164914293175,"d":"2.28"},{"v":2.2801649142931755,"d":"2.28"},{"v":0.7505544189999999,"d":"0.75"}]
["27103","Nicollet","MN",{"v":0.271827368,"d":"0.27"},{"v":2.172542124704441,"d":"2.17"},{"v":2.172542124704441,"d":"2.17"},{"v":0.65332132,"d":"0.65"}]
["27105","Nobles","MN",{"v":0.292043464,"d":"0.29"},{"v":2.2350549149215078,"d":"2.24"},{"v":2.2350549149215078,"d":"2.24"},{"v":0.677522547,"d":"0.68"}]
["27107","Norman","MN",{"v":0.31974173,"d":"0.32"},{"v":2.410935906472703,"d":"2.41"},{"v":2.410935906472703,"d":"2.41"},{"v":0.7912872765,"d":"0.79"}]
["27109","Olmsted","MN",{"v":0.252677328,"d":"0.25"},{"v":2.1434736833909893,"d":"2.14"},{"v":2.1434736833909893,"d":"2.14"},{"v":0.6377626670000001,"d":"0.64"}]
["27111","Otter Tail","MN",{"v":0.300515688,"d":"0.30"},{"v":2.333179270977686,"d":"2.33"},{"v":2.333179270977686,"d":"2.33"},{"v":0.7619941039999999,"d":"0.76"}]
["27113","Pennington","MN",{"v":0.262402158,"d":"0.26"},{"v":2.354361852692599,"d":"2.35"},{"v":2.354361852692599,"d":"2.35"},{"v":0.704770065,"d":"0.70"}]
["27115","Pine","MN",{"v":0.292748968,"d":"0.29"},{"v":2.446415454817039,"d":"2.45"},{"v":2.446415454817039,"d":"2.45"},{"v":0.8935149265,"d":"0.89"}]
["27117","Pipestone","MN",{"v":0.2977479860000001,"d":"0.30"},{"v":2.2401365072909947,"d":"2.24"},{"v":2.2401365072909947,"d":"2.24"},{"v":0.695916543,"d":"0.70"}]
["27119","Polk","MN",{"v":0.278765713,"d":"0.28"},{"v":2.3794907513628707,"d":"2.38"},{"v":2.379490751362871,"d":"2.38"},{"v":0.724342631,"d":"0.72"}]
["27121","Pope","MN",{"v":0.335456284,"d":"0.34"},{"v":2.3088147568202166,"d":"2.31"},{"v":2.308814756820216,"d":"2.31"},{"v":0.7701460765,"d":"0.77"}]
["27123","Ramsey","MN",{"v":0.07756336499999998,"d":"0.08"},{"v":3.40391886424719E-4,"d":"0.00"},{"v":3.4039188642471905E-4,"d":"0.00"},{"v":0.45550786600000004,"d":"0.46"}]
["27125","Red Lake","MN",{"v":0.318720998,"d":"0.32"},{"v":2.411499475849674,"d":"2.41"},{"v":2.4114994758496744,"d":"2.41"},{"v":0.8034976079999999,"d":"0.80"}]
["27127","Redwood","MN",{"v":0.307926631,"d":"0.31"},{"v":2.2573252314016763,"d":"2.26"},{"v":2.2573252314016763,"d":"2.26"},{"v":0.7159270100000001,"d":"0.72"}]
["27129","Renville","MN",{"v":0.331652951,"d":"0.33"},{"v":2.273575696333928,"d":"2.27"},{"v":2.273575696333928,"d":"2.27"},{"v":0.7589713365,"d":"0.76"}]
["27131","Rice","MN",{"v":0.267657373,"d":"0.27"},{"v":2.1813623680399945,"d":"2.18"},{"v":2.1813623680399945,"d":"2.18"},{"v":0.6633908365,"d":"0.66"}]
["27133","Rock","MN",{"v":0.296978167,"d":"0.30"},{"v":2.2370615408299557,"d":"2.24"},{"v":2.2370615408299552,"d":"2.24"},{"v":0.688483234,"d":"0.69"}]
["27135","Roseau","MN",{"v":0.29582189999999997,"d":"0.30"},{"v":2.453023501008084,"d":"2.45"},{"v":2.453023501008084,"d":"2.45"},{"v":0.8096031220000001,"d":"0.81"}]
["27137","St Louis","MN",{"v":0.24669559500000002,"d":"0.25"},{"v":2.4695177433593094,"d":"2.47"},{"v":2.469517743359309,"d":"2.47"},{"v":0.8290893215000001,"d":"0.83"}]
["27139","Scott","MN",{"v":0.250116433,"d":"0.25"},{"v":2.189334203070272,"d":"2.19"},{"v":2.189334203070272,"d":"2.19"},{"v":0.6343096229999999,"d":"0.63"}]
["27141","Sherburne","MN",{"v":0.26537027,"d":"0.27"},{"v":2.2352028183733874,"d":"2.24"},{"v":2.235202818373387,"d":"2.24"},{"v":0.7170719299999999,"d":"0.72"}]
["27143","Sibley","MN",{"v":0.334781602,"d":"0.33"},{"v":2.272840636809306,"d":"2.27"},{"v":2.272840636809306,"d":"2.27"},{"v":0.7623074160000001,"d":"0.76"}]
["27145","Stearns","MN",{"v":0.263083715,"d":"0.26"},{"v":2.2478796435070523,"d":"2.25"},{"v":2.2478796435070523,"d":"2.25"},{"v":0.686095083,"d":"0.69"}]
["27147","Steele","MN",{"v":0.27449802,"d":"0.27"},{"v":2.157686037227741,"d":"2.16"},{"v":2.157686037227741,"d":"2.16"},{"v":0.6571065739999999,"d":"0.66"}]
["27149","Stevens","MN",{"v":0.28611524099999996,"d":"0.29"},{"v":2.2502201457370496,"d":"2.25"},{"v":2.250220145737049,"d":"2.25"},{"v":0.6964687115,"d":"0.70"}]
["27151","Swift","MN",{"v":0.305323647,"d":"0.31"},{"v":2.2860579952839255,"d":"2.29"},{"v":2.286057995283926,"d":"2.29"},{"v":0.7212055725000001,"d":"0.72"}]
["27153","Todd","MN",{"v":0.30653249199999993,"d":"0.31"},{"v":2.332460335666817,"d":"2.33"},{"v":2.3324603356668168,"d":"2.33"},{"v":0.7793400105,"d":"0.78"}]
["27155","Traverse","MN",{"v":0.3332056239999999,"d":"0.33"},{"v":2.3274046264039225,"d":"2.33"},{"v":2.327404626403923,"d":"2.33"},{"v":0.7588042084999999,"d":"0.76"}]
["27157","Wabasha","MN",{"v":0.294729482,"d":"0.29"},{"v":2.2474426300458257,"d":"2.25"},{"v":2.2474426300458257,"d":"2.25"},{"v":0.7633440085,"d":"0.76"}]
["27159","Wadena","MN",{"v":0.293099754,"d":"0.29"},{"v":2.3237793088506096,"d":"2.32"},{"v":2.3237793088506096,"d":"2.32"},{"v":0.770819668,"d":"0.77"}]
["27161","Waseca","MN",{"v":0.291108086,"d":"0.29"},{"v":2.1933062023554544,"d":"2.19"},{"v":2.1933062023554544,"d":"2.19"},{"v":0.6940162429999998,"d":"0.69"}]
["27163","Washington","MN",{"v":0.223473319,"d":"0.22"},{"v":2.1233699605068757,"d":"2.12"},{"v":2.1233699605068757,"d":"2.12"},{"v":0.6345635895,"d":"0.63"}]
["27165","Watonwan","MN",{"v":0.300341248,"d":"0.30"},{"v":2.178584436011715,"d":"2.18"},{"v":2.178584436011715,"d":"2.18"},{"v":0.7050278470000001,"d":"0.71"}]
["27167","Wilkin","MN",{"v":0.292679315,"d":"0.29"},{"v":2.2957873595335188,"d":"2.30"},{"v":2.2957873595335183,"d":"2.30"},{"v":0.695121094,"d":"0.70"}]
["27169","Winona","MN",{"v":0.259263845,"d":"0.26"},{"v":2.2060297996041105,"d":"2.21"},{"v":2.206029799604111,"d":"2.21"},{"v":0.7466415550000001,"d":"0.75"}]
["27171","Wright","MN",{"v":0.268503997,"d":"0.27"},{"v":2.235884216045812,"d":"2.24"},{"v":2.2358842160458114,"d":"2.24"},{"v":0.6755034855000001,"d":"0.68"}]
["27173","Yellow Medicine","MN",{"v":0.315259751,"d":"0.32"},{"v":2.2824611609721837,"d":"2.28"},{"v":2.282461160972183,"d":"2.28"},{"v":0.7394552014999999,"d":"0.74"}]
["28001","Adams","MS",{"v":0.24635752800000002,"d":"0.25"},{"v":1.481562027851935,"d":"1.48"},{"v":1.4815620278519352,"d":"1.48"},{"v":0.721253006,"d":"0.72"}]
["28003","Alcorn","MS",{"v":0.265985554,"d":"0.27"},{"v":1.6159351834426292,"d":"1.62"},{"v":1.6159351834426292,"d":"1.62"},{"v":0.76611312,"d":"0.77"}]
["28005","Amite","MS",{"v":0.29407468,"d":"0.29"},{"v":1.651393953610321,"d":"1.65"},{"v":1.651393953610321,"d":"1.65"},{"v":0.8467202085,"d":"0.85"}]
["28007","Attala","MS",{"v":0.264144086,"d":"0.26"},{"v":1.5710278175620778,"d":"1.57"},{"v":1.5710278175620778,"d":"1.57"},{"v":0.8243649514999999,"d":"0.82"}]
["28009","Benton","MS",{"v":0.294186937,"d":"0.29"},{"v":1.6656054113123415,"d":"1.67"},{"v":1.6656054113123417,"d":"1.67"},{"v":0.8160388395,"d":"0.82"}]
["28011","Bolivar","MS",{"v":0.29366009200000004,"d":"0.29"},{"v":1.503466762091291,"d":"1.50"},{"v":1.503466762091291,"d":"1.50"},{"v":0.5881839194999999,"d":"0.59"}]
["28013","Calhoun","MS",{"v":0.297957644,"d":"0.30"},{"v":1.651017876592733,"d":"1.65"},{"v":1.651017876592733,"d":"1.65"},{"v":0.794030721,"d":"0.79"}]
["28015","Carroll","MS",{"v":0.296579075,"d":"0.30"},{"v":1.6733428212484538,"d":"1.67"},{"v":1.6733428212484536,"d":"1.67"},{"v":0.8139102645,"d":"0.81"}]
["28017","Chickasaw","MS",{"v":0.29438644100000005,"d":"0.29"},{"v":1.6237075203815305,"d":"1.62"},{"v":1.623707520381531,"d":"1.62"},{"v":0.7255624439999999,"d":"0.73"}]
["28019","Choctaw","MS",{"v":0.28684191,"d":"0.29"},{"v":1.6244712598035467,"d":"1.62"},{"v":1.6244712598035467,"d":"1.62"},{"v":0.880680794,"d":"0.88"}]
["28021","Claiborne","MS",{"v":0.284452921,"d":"0.28"},{"v":1.6230914765563416,"d":"1.62"},{"v":1.6230914765563416,"d":"1.62"},{"v":0.8425597125000001,"d":"0.84"}]
["28023","Clarke","MS",{"v":0.293646233,"d":"0.29"},{"v":1.5995273865976176,"d":"1.60"},{"v":1.5995273865976176,"d":"1.60"},{"v":0.8479581975,"d":"0.85"}]
["28025","Clay","MS",{"v":0.272474431,"d":"0.27"},{"v":1.5458681254858033,"d":"1.55"},{"v":1.5458681254858033,"d":"1.55"},{"v":0.701959778,"d":"0.70"}]
["28027","Coahoma","MS",{"v":0.272054821,"d":"0.27"},{"v":1.4932757375682963,"d":"1.49"},{"v":1.4932757375682963,"d":"1.49"},{"v":0.5641150105000001,"d":"0.56"}]
["28029","Copiah","MS",{"v":0.269151519,"d":"0.27"},{"v":1.5744982887398056,"d":"1.57"},{"v":1.5744982887398054,"d":"1.57"},{"v":0.8020312995,"d":"0.80"}]
["28031","Covington","MS",{"v":0.298181803,"d":"0.30"},{"v":1.5938450867238196,"d":"1.59"},{"v":1.5938450867238196,"d":"1.59"},{"v":0.8027867994999999,"d":"0.80"}]
["28033","De Soto","MS",{"v":0.22962798699999995,"d":"0.23"},{"v":1.5079139487473876,"d":"1.51"},{"v":1.5079139487473878,"d":"1.51"},{"v":0.5899793440000001,"d":"0.59"}]
["28035","Forrest","MS",{"v":0.23489812799999998,"d":"0.23"},{"v":1.504354278026034,"d":"1.50"},{"v":1.504354278026034,"d":"1.50"},{"v":0.7071943900000001,"d":"0.71"}]
["28037","Franklin","MS",{"v":0.289455133,"d":"0.29"},{"v":1.6062763728193432,"d":"1.61"},{"v":1.606276372819343,"d":"1.61"},{"v":0.8914001385000002,"d":"0.89"}]
["28039","George","MS",{"v":0.295840539,"d":"0.30"},{"v":1.5877481150597703,"d":"1.59"},{"v":1.5877481150597705,"d":"1.59"},{"v":0.7835917385000001,"d":"0.78"}]
["28041","Greene","MS",{"v":0.296221706,"d":"0.30"},{"v":1.6305619214714329,"d":"1.63"},{"v":1.630561921471433,"d":"1.63"},{"v":0.8439224035,"d":"0.84"}]
["28043","Grenada","MS",{"v":0.260542653,"d":"0.26"},{"v":1.588009242699387,"d":"1.59"},{"v":1.5880092426993866,"d":"1.59"},{"v":0.7427575344999999,"d":"0.74"}]
["28045","Hancock","MS",{"v":0.268601323,"d":"0.27"},{"v":1.550543970361355,"d":"1.55"},{"v":1.5505439703613548,"d":"1.55"},{"v":0.6452549895,"d":"0.65"}]
["28047","Harrison","MS",{"v":0.23690794099999998,"d":"0.24"},{"v":1.469673567330405,"d":"1.47"},{"v":1.469673567330405,"d":"1.47"},{"v":0.559514833,"d":"0.56"}]
["28049","Hinds","MS",{"v":0.222077872,"d":"0.22"},{"v":1.426633033510878,"d":"1.43"},{"v":1.426633033510878,"d":"1.43"},{"v":0.661693736,"d":"0.66"}]
["28051","Holmes","MS",{"v":0.287411002,"d":"0.29"},{"v":1.5939375137133203,"d":"1.59"},{"v":1.59393751371332,"d":"1.59"},{"v":0.7661220335,"d":"0.77"}]
["28053","Humphreys","MS",{"v":0.299121472,"d":"0.30"},{"v":1.48741902479133,"d":"1.49"},{"v":1.48741902479133,"d":"1.49"},{"v":0.577659762,"d":"0.58"}]
["28055","Issaquena","MS",{"v":0.295925838,"d":"0.30"},{"v":1.6851630866271574,"d":"1.69"},{"v":1.6851630866271576,"d":"1.69"},{"v":0.7110216380000001,"d":"0.71"}]
["28057","Itawamba","MS",{"v":0.281837718,"d":"0.28"},{"v":1.6542305033561173,"d":"1.65"},{"v":1.6542305033561175,"d":"1.65"},{"v":0.819384429,"d":"0.82"}]
["28059","Jackson","MS",{"v":0.252549873,"d":"0.25"},{"v":1.515673813344734,"d":"1.52"},{"v":1.5156738133447338,"d":"1.52"},{"v":0.5830392615000001,"d":"0.58"}]
["28061","Jasper","MS",{"v":0.29433452299999996,"d":"0.29"},{"v":1.644184670671942,"d":"1.64"},{"v":1.644184670671942,"d":"1.64"},{"v":0.8432291314999999,"d":"0.84"}]
["28063","Jefferson","MS",{"v":0.291652254,"d":"0.29"},{"v":1.5916646151195264,"d":"1.59"},{"v":1.5916646151195266,"d":"1.59"},{"v":0.8643547604999999,"d":"0.86"}]
["28065","Jefferson Davis","MS",{"v":0.29844682199999994,"d":"0.30"},{"v":1.6192090544787021,"d":"1.62"},{"v":1.6192090544787021,"d":"1.62"},{"v":0.8146181155,"d":"0.81"}]
["28067","Jones","MS",{"v":0.266374902,"d":"0.27"},{"v":1.5548395797629173,"d":"1.55"},{"v":1.5548395797629175,"d":"1.55"},{"v":0.7589868439999999,"d":"0.76"}]
["28069","Kemper","MS",{"v":0.295547358,"d":"0.30"},{"v":1.645344583872163,"d":"1.65"},{"v":1.6453445838721628,"d":"1.65"},{"v":0.8439459280000001,"d":"0.84"}]
["28071","Lafayette","MS",{"v":0.24503947899999998,"d":"0.25"},{"v":1.6144510621874977,"d":"1.61"},{"v":1.6144510621874977,"d":"1.61"},{"v":0.7664226465,"d":"0.77"}]
["28073","Lamar","MS",{"v":0.251610276,"d":"0.25"},{"v":1.5389553062405017,"d":"1.54"},{"v":1.5389553062405017,"d":"1.54"},{"v":0.7484124955000001,"d":"0.75"}]
["28075","Lauderdale","MS",{"v":0.250336854,"d":"0.25"},{"v":1.5267599814932609,"d":"1.53"},{"v":1.5267599814932606,"d":"1.53"},{"v":0.768717691,"d":"0.77"}]
["28077","Lawrence","MS",{"v":0.29732779500000006,"d":"0.30"},{"v":1.617172688354571,"d":"1.62"},{"v":1.617172688354571,"d":"1.62"},{"v":0.8184794655,"d":"0.82"}]
["28079","Leake","MS",{"v":0.278923673,"d":"0.28"},{"v":1.656192569444184,"d":"1.66"},{"v":1.656192569444184,"d":"1.66"},{"v":0.824569139,"d":"0.82"}]
["28081","Lee","MS",{"v":0.250040032,"d":"0.25"},{"v":1.5664904208309354,"d":"1.57"},{"v":1.5664904208309356,"d":"1.57"},{"v":0.663395579,"d":"0.66"}]
["28083","Leflore","MS",{"v":0.26946014499999993,"d":"0.27"},{"v":1.4061287951935282,"d":"1.41"},{"v":1.4061287951935282,"d":"1.41"},{"v":0.539875673,"d":"0.54"}]
["28085","Lincoln","MS",{"v":0.273663699,"d":"0.27"},{"v":1.589051437010456,"d":"1.59"},{"v":1.589051437010456,"d":"1.59"},{"v":0.779440582,"d":"0.78"}]
["28087","Lowndes","MS",{"v":0.25797953,"d":"0.26"},{"v":1.5538509835876657,"d":"1.55"},{"v":1.5538509835876657,"d":"1.55"},{"v":0.6731196395000002,"d":"0.67"}]
["28089","Madison","MS",{"v":0.241125167,"d":"0.24"},{"v":1.4941259235032847,"d":"1.49"},{"v":1.4941259235032847,"d":"1.49"},{"v":0.6711541414999999,"d":"0.67"}]
["28091","Marion","MS",{"v":0.276905493,"d":"0.28"},{"v":1.6038212344559208,"d":"1.60"},{"v":1.6038212344559206,"d":"1.60"},{"v":0.7795780409999998,"d":"0.78"}]
["28093","Marshall","MS",{"v":0.284434243,"d":"0.28"},{"v":1.6678298635854487,"d":"1.67"},{"v":1.6678298635854492,"d":"1.67"},{"v":0.7709914710000002,"d":"0.77"}]
["28095","Monroe","MS",{"v":0.279378794,"d":"0.28"},{"v":1.601315731688956,"d":"1.60"},{"v":1.6013157316889557,"d":"1.60"},{"v":0.7314593829999999,"d":"0.73"}]
["28097","Montgomery","MS",{"v":0.26973545600000004,"d":"0.27"},{"v":1.5224056369165457,"d":"1.52"},{"v":1.5224056369165453,"d":"1.52"},{"v":0.7970401069999999,"d":"0.80"}]
["28099","Neshoba","MS",{"v":0.271774079,"d":"0.27"},{"v":1.6514457110025798,"d":"1.65"},{"v":1.6514457110025798,"d":"1.65"},{"v":0.8024044555000001,"d":"0.80"}]
["28101","Newton","MS",{"v":0.28459722800000004,"d":"0.28"},{"v":1.584525793025507,"d":"1.58"},{"v":1.5845257930255072,"d":"1.58"},{"v":0.8232084999999999,"d":"0.82"}]
["28103","Noxubee","MS",{"v":0.280741334,"d":"0.28"},{"v":1.6659384236373598,"d":"1.67"},{"v":1.6659384236373602,"d":"1.67"},{"v":0.7307514460000001,"d":"0.73"}]
["28105","Oktibbeha","MS",{"v":0.238868129,"d":"0.24"},{"v":1.5111544959377885,"d":"1.51"},{"v":1.511154495937789,"d":"1.51"},{"v":0.7404130320000001,"d":"0.74"}]
["28107","Panola","MS",{"v":0.289789516,"d":"0.29"},{"v":1.6772632991148972,"d":"1.68"},{"v":1.677263299114897,"d":"1.68"},{"v":0.7041760304999999,"d":"0.70"}]
["28109","Pearl River","MS",{"v":0.278147992,"d":"0.28"},{"v":1.5610279616557434,"d":"1.56"},{"v":1.5610279616557434,"d":"1.56"},{"v":0.754146576,"d":"0.75"}]
["28111","Perry","MS",{"v":0.29252387899999993,"d":"0.29"},{"v":1.6567765293832832,"d":"1.66"},{"v":1.6567765293832835,"d":"1.66"},{"v":0.8392972830000001,"d":"0.84"}]
["28113","Pike","MS",{"v":0.265207288,"d":"0.27"},{"v":1.5519386920805018,"d":"1.55"},{"v":1.551938692080502,"d":"1.55"},{"v":0.7425691744999999,"d":"0.74"}]
["28115","Pontotoc","MS",{"v":0.286809943,"d":"0.29"},{"v":1.6393297331789423,"d":"1.64"},{"v":1.639329733178942,"d":"1.64"},{"v":0.748271517,"d":"0.75"}]
["28117","Prentiss","MS",{"v":0.279989612,"d":"0.28"},{"v":1.599395109028041,"d":"1.60"},{"v":1.5993951090280407,"d":"1.60"},{"v":0.769769936,"d":"0.77"}]
["28119","Quitman","MS",{"v":0.30056971800000004,"d":"0.30"},{"v":1.5597488096818966,"d":"1.56"},{"v":1.5597488096818966,"d":"1.56"},{"v":0.5964016955,"d":"0.60"}]
["28121","Rankin","MS",{"v":0.236828275,"d":"0.24"},{"v":1.5252938919749282,"d":"1.53"},{"v":1.5252938919749286,"d":"1.53"},{"v":0.7197913764999999,"d":"0.72"}]
["28123","Scott","MS",{"v":0.272412171,"d":"0.27"},{"v":1.6525708029219583,"d":"1.65"},{"v":1.6525708029219586,"d":"1.65"},{"v":0.8139035840000001,"d":"0.81"}]
["28125","Sharkey","MS",{"v":0.323295094,"d":"0.32"},{"v":1.4992568193719868,"d":"1.50"},{"v":1.4992568193719866,"d":"1.50"},{"v":0.689557405,"d":"0.69"}]
["28127","Simpson","MS",{"v":0.28594164899999996,"d":"0.29"},{"v":1.6081480451665418,"d":"1.61"},{"v":1.6081480451665418,"d":"1.61"},{"v":0.806305969,"d":"0.81"}]
["28129","Smith","MS",{"v":0.293500024,"d":"0.29"},{"v":1.6195582779271631,"d":"1.62"},{"v":1.619558277927163,"d":"1.62"},{"v":0.8489381574999998,"d":"0.85"}]
["28131","Stone","MS",{"v":0.284818013,"d":"0.28"},{"v":1.559720162067885,"d":"1.56"},{"v":1.5597201620678849,"d":"1.56"},{"v":0.79932785,"d":"0.80"}]
["28133","Sunflower","MS",{"v":0.28998039300000006,"d":"0.29"},{"v":1.4350434002364936,"d":"1.44"},{"v":1.4350434002364931,"d":"1.44"},{"v":0.5424437129999999,"d":"0.54"}]
["28135","Tallahatchie","MS",{"v":0.303453511,"d":"0.30"},{"v":1.659986329894517,"d":"1.66"},{"v":1.659986329894517,"d":"1.66"},{"v":0.6577855270000001,"d":"0.66"}]
["28137","Tate","MS",{"v":0.288751935,"d":"0.29"},{"v":1.6456709716635451,"d":"1.65"},{"v":1.6456709716635451,"d":"1.65"},{"v":0.7021147404999999,"d":"0.70"}]
["28139","Tippah","MS",{"v":0.280872561,"d":"0.28"},{"v":1.605789765589888,"d":"1.61"},{"v":1.605789765589888,"d":"1.61"},{"v":0.796001668,"d":"0.80"}]
["28141","Tishomingo","MS",{"v":0.290621639,"d":"0.29"},{"v":1.6401221554796865,"d":"1.64"},{"v":1.6401221554796868,"d":"1.64"},{"v":0.8270476104999999,"d":"0.83"}]
["28143","Tunica","MS",{"v":0.28119476,"d":"0.28"},{"v":1.6020842717359793,"d":"1.60"},{"v":1.6020842717359793,"d":"1.60"},{"v":0.6168299450000001,"d":"0.62"}]
["28145","Union","MS",{"v":0.277722411,"d":"0.28"},{"v":1.5866959006473764,"d":"1.59"},{"v":1.5866959006473766,"d":"1.59"},{"v":0.7514890985,"d":"0.75"}]
["28147","Walthall","MS",{"v":0.30459319,"d":"0.30"},{"v":1.6262212624835457,"d":"1.63"},{"v":1.6262212624835455,"d":"1.63"},{"v":0.7679022354999999,"d":"0.77"}]
["28149","Warren","MS",{"v":0.246960906,"d":"0.25"},{"v":1.5435802175092395,"d":"1.54"},{"v":1.5435802175092395,"d":"1.54"},{"v":0.731549057,"d":"0.73"}]
["28151","Washington","MS",{"v":0.264851478,"d":"0.26"},{"v":1.4360751046786988,"d":"1.44"},{"v":1.4360751046786988,"d":"1.44"},{"v":0.5342519185,"d":"0.53"}]
["28153","Wayne","MS",{"v":0.276200834,"d":"0.28"},{"v":1.6105669132869582,"d":"1.61"},{"v":1.610566913286958,"d":"1.61"},{"v":0.8202053954999999,"d":"0.82"}]
["28155","Webster","MS",{"v":0.293069943,"d":"0.29"},{"v":1.5979656417301635,"d":"1.60"},{"v":1.5979656417301635,"d":"1.60"},{"v":0.8334076975000002,"d":"0.83"}]
["28157","Wilkinson","MS",{"v":0.2897772960000001,"d":"0.29"},{"v":1.6527180035890965,"d":"1.65"},{"v":1.6527180035890963,"d":"1.65"},{"v":0.8567989169999999,"d":"0.86"}]
["28159","Winston","MS",{"v":0.274131263,"d":"0.27"},{"v":1.6056988438883435,"d":"1.61"},{"v":1.6056988438883435,"d":"1.61"},{"v":0.8370988985000002,"d":"0.84"}]
["28161","Yalobusha","MS",{"v":0.278617736,"d":"0.28"},{"v":1.672173821621251,"d":"1.67"},{"v":1.672173821621251,"d":"1.67"},{"v":0.7865432019999999,"d":"0.79"}]
["28163","Yazoo","MS",{"v":0.271038465,"d":"0.27"},{"v":1.5595386670913494,"d":"1.56"},{"v":1.5595386670913494,"d":"1.56"},{"v":0.7005781655,"d":"0.70"}]
["29001","Adair","MO",{"v":0.7223577829999999,"d":"0.72"},{"v":4.735024981181241,"d":"4.74"},{"v":4.735024981181241,"d":"4.74"},{"v":1.6670927445,"d":"1.67"}]
["29003","Andrew","MO",{"v":0.780474467,"d":"0.78"},{"v":4.935321716612162,"d":"4.94"},{"v":4.935321716612162,"d":"4.94"},{"v":1.6743386634999997,"d":"1.67"}]
["29005","Atchison","MO",{"v":0.891704746,"d":"0.89"},{"v":4.856989259445851,"d":"4.86"},{"v":4.856989259445851,"d":"4.86"},{"v":1.7281775995000002,"d":"1.73"}]
["29007","Audrain","MO",{"v":0.748954497,"d":"0.75"},{"v":4.669224335757674,"d":"4.67"},{"v":4.669224335757675,"d":"4.67"},{"v":1.5869918190000003,"d":"1.59"}]
["29009","Barry","MO",{"v":0.766570142,"d":"0.77"},{"v":4.824327108735245,"d":"4.82"},{"v":4.824327108735245,"d":"4.82"},{"v":1.9005641625,"d":"1.90"}]
["29011","Barton","MO",{"v":0.816292371,"d":"0.82"},{"v":4.64619536016978,"d":"4.65"},{"v":4.64619536016978,"d":"4.65"},{"v":1.626825532,"d":"1.63"}]
["29013","Bates","MO",{"v":0.8350552290000001,"d":"0.84"},{"v":4.7536460034470664,"d":"4.75"},{"v":4.7536460034470664,"d":"4.75"},{"v":1.6915167990000002,"d":"1.69"}]
["29015","Benton","MO",{"v":0.798038388,"d":"0.80"},{"v":5.04318299957925,"d":"5.04"},{"v":5.04318299957925,"d":"5.04"},{"v":1.9186738205000005,"d":"1.92"}]
["29017","Bollinger","MO",{"v":0.808123261,"d":"0.81"},{"v":4.979708915912856,"d":"4.98"},{"v":4.979708915912855,"d":"4.98"},{"v":2.0602348105,"d":"2.06"}]
["29019","Boone","MO",{"v":0.6132439960000001,"d":"0.61"},{"v":4.519353033861818,"d":"4.52"},{"v":4.519353033861818,"d":"4.52"},{"v":1.622898762,"d":"1.62"}]
["29021","Buchanan","MO",{"v":0.630591377,"d":"0.63"},{"v":4.642331650473805,"d":"4.64"},{"v":4.642331650473805,"d":"4.64"},{"v":1.5027472615000004,"d":"1.50"}]
["29023","Butler","MO",{"v":0.740106384,"d":"0.74"},{"v":4.594932506432571,"d":"4.59"},{"v":4.594932506432571,"d":"4.59"},{"v":1.7373526264999999,"d":"1.74"}]
["29025","Caldwell","MO",{"v":0.865258562,"d":"0.87"},{"v":5.088119649391295,"d":"5.09"},{"v":5.088119649391295,"d":"5.09"},{"v":1.787343234,"d":"1.79"}]
["29027","Callaway","MO",{"v":0.746026877,"d":"0.75"},{"v":4.9422022142327195,"d":"4.94"},{"v":4.9422022142327195,"d":"4.94"},{"v":1.8655375420000002,"d":"1.87"}]
["29029","Camden","MO",{"v":0.704827536,"d":"0.70"},{"v":5.0023527224660835,"d":"5.00"},{"v":5.0023527224660835,"d":"5.00"},{"v":2.0162196480000003,"d":"2.02"}]
["29031","Cape Girardeau","MO",{"v":0.6771372900000001,"d":"0.68"},{"v":4.565952101684096,"d":"4.57"},{"v":4.565952101684097,"d":"4.57"},{"v":1.618368921,"d":"1.62"}]
["29033","Carroll","MO",{"v":0.781313145,"d":"0.78"},{"v":4.871193384834038,"d":"4.87"},{"v":4.871193384834038,"d":"4.87"},{"v":1.69377484,"d":"1.69"}]
["29035","Carter","MO",{"v":0.750160401,"d":"0.75"},{"v":5.157399330953848,"d":"5.16"},{"v":5.157399330953849,"d":"5.16"},{"v":2.4419615364999996,"d":"2.44"}]
["29037","Cass","MO",{"v":0.7270727320000001,"d":"0.73"},{"v":4.53265362176969,"d":"4.53"},{"v":4.53265362176969,"d":"4.53"},{"v":1.5307035044999997,"d":"1.53"}]
["29039","Cedar","MO",{"v":0.786527103,"d":"0.79"},{"v":4.869733125392432,"d":"4.87"},{"v":4.869733125392431,"d":"4.87"},{"v":1.8377276880000002,"d":"1.84"}]
["29041","Chariton","MO",{"v":0.864290076,"d":"0.86"},{"v":4.985905532423758,"d":"4.99"},{"v":4.985905532423759,"d":"4.99"},{"v":1.7935885985000002,"d":"1.79"}]
["29043","Christian","MO",{"v":0.695387302,"d":"0.70"},{"v":4.619536346212975,"d":"4.62"},{"v":4.619536346212975,"d":"4.62"},{"v":1.799169194,"d":"1.80"}]
["29045","Clark","MO",{"v":0.859245603,"d":"0.86"},{"v":4.99241703227823,"d":"4.99"},{"v":4.992417032278231,"d":"4.99"},{"v":1.822399043,"d":"1.82"}]
["29047","Clay","MO",{"v":0.554140049,"d":"0.55"},{"v":4.386415706496594,"d":"4.39"},{"v":4.386415706496594,"d":"4.39"},{"v":1.413671108,"d":"1.41"}]
["29049","Clinton","MO",{"v":0.8153496150000001,"d":"0.82"},{"v":4.83557292124848,"d":"4.84"},{"v":4.83557292124848,"d":"4.84"},{"v":1.7098419819999997,"d":"1.71"}]
["29051","Cole","MO",{"v":0.662683837,"d":"0.66"},{"v":4.605323009860383,"d":"4.61"},{"v":4.605323009860383,"d":"4.61"},{"v":1.6670064805000002,"d":"1.67"}]
["29053","Cooper","MO",{"v":0.7697987419999999,"d":"0.77"},{"v":4.649756667201292,"d":"4.65"},{"v":4.649756667201293,"d":"4.65"},{"v":1.6811158855,"d":"1.68"}]
["29055","Crawford","MO",{"v":0.742376942,"d":"0.74"},{"v":4.9452297161905765,"d":"4.95"},{"v":4.9452297161905765,"d":"4.95"},{"v":2.0343226370000003,"d":"2.03"}]
["29057","Dade","MO",{"v":0.873661361,"d":"0.87"},{"v":4.758635313023026,"d":"4.76"},{"v":4.758635313023026,"d":"4.76"},{"v":1.781986998,"d":"1.78"}]
["29059","Dallas","MO",{"v":0.7888427690000002,"d":"0.79"},{"v":4.975677058951507,"d":"4.98"},{"v":4.975677058951507,"d":"4.98"},{"v":1.8965126475,"d":"1.90"}]
["29061","Daviess","MO",{"v":0.862385564,"d":"0.86"},{"v":4.998420128601854,"d":"5.00"},{"v":4.998420128601854,"d":"5.00"},{"v":1.7872731880000001,"d":"1.79"}]
["29063","Dekalb","MO",{"v":0.8345128460000002,"d":"0.83"},{"v":4.990630570579877,"d":"4.99"},{"v":4.990630570579877,"d":"4.99"},{"v":1.7287119230000003,"d":"1.73"}]
["29065","Dent","MO",{"v":0.7387267739999999,"d":"0.74"},{"v":4.9698768568041825,"d":"4.97"},{"v":4.9698768568041825,"d":"4.97"},{"v":2.031147749,"d":"2.03"}]
["29067","Douglas","MO",{"v":0.7585826019999999,"d":"0.76"},{"v":4.889866965584391,"d":"4.89"},{"v":4.889866965584391,"d":"4.89"},{"v":2.0381616295,"d":"2.04"}]
["29069","Dunklin","MO",{"v":0.795386012,"d":"0.80"},{"v":4.283111606935339,"d":"4.28"},{"v":4.283111606935339,"d":"4.28"},{"v":1.530363683,"d":"1.53"}]
["29071","Franklin","MO",{"v":0.695986914,"d":"0.70"},{"v":5.0542373814423796,"d":"5.05"},{"v":5.0542373814423796,"d":"5.05"},{"v":1.900812407,"d":"1.90"}]
["29073","Gasconade","MO",{"v":0.764595277,"d":"0.76"},{"v":5.06695936569686,"d":"5.07"},{"v":5.06695936569686,"d":"5.07"},{"v":2.0205603594999997,"d":"2.02"}]
["29075","Gentry","MO",{"v":0.8711156300000001,"d":"0.87"},{"v":4.928745944100978,"d":"4.93"},{"v":4.928745944100978,"d":"4.93"},{"v":1.7690999620000003,"d":"1.77"}]
["29077","Greene","MO",{"v":0.590743063,"d":"0.59"},{"v":4.287883561963247,"d":"4.29"},{"v":4.287883561963247,"d":"4.29"},{"v":1.4547710154999998,"d":"1.45"}]
["29079","Grundy","MO",{"v":0.7527000380000001,"d":"0.75"},{"v":4.916106269146821,"d":"4.92"},{"v":4.916106269146821,"d":"4.92"},{"v":1.6256562785000002,"d":"1.63"}]
["29081","Harrison","MO",{"v":0.7971417789999999,"d":"0.80"},{"v":4.913827716298901,"d":"4.91"},{"v":4.913827716298901,"d":"4.91"},{"v":1.7150959865,"d":"1.72"}]
["29083","Henry","MO",{"v":0.75508037,"d":"0.76"},{"v":4.739911584819955,"d":"4.74"},{"v":4.739911584819955,"d":"4.74"},{"v":1.6477554984999998,"d":"1.65"}]
["29085","Hickory","MO",{"v":0.8135055440000001,"d":"0.81"},{"v":5.158772005155643,"d":"5.16"},{"v":5.158772005155642,"d":"5.16"},{"v":1.998670898,"d":"2.00"}]
["29087","Holt","MO",{"v":0.88213893,"d":"0.88"},{"v":4.914703934977192,"d":"4.91"},{"v":4.914703934977192,"d":"4.91"},{"v":1.7605411999999998,"d":"1.76"}]
["29089","Howard","MO",{"v":0.7629886570000001,"d":"0.76"},{"v":4.9313289021347835,"d":"4.93"},{"v":4.9313289021347835,"d":"4.93"},{"v":1.8006732965000003,"d":"1.80"}]
["29091","Howell","MO",{"v":0.746242111,"d":"0.75"},{"v":4.852617862054848,"d":"4.85"},{"v":4.852617862054849,"d":"4.85"},{"v":1.9308204935,"d":"1.93"}]
["29093","Iron","MO",{"v":0.716688499,"d":"0.72"},{"v":4.938501705341946,"d":"4.94"},{"v":4.938501705341946,"d":"4.94"},{"v":2.265095928,"d":"2.27"}]
["29095","Jackson","MO",{"v":0.45561310399999994,"d":"0.46"},{"v":2.7226190474621492,"d":"2.72"},{"v":2.7226190474621497,"d":"2.72"},{"v":1.3412917574999998,"d":"1.34"}]
["29097","Jasper","MO",{"v":0.678461072,"d":"0.68"},{"v":4.447426868047689,"d":"4.45"},{"v":4.447426868047689,"d":"4.45"},{"v":1.502340938,"d":"1.50"}]
["29099","Jefferson","MO",{"v":0.6031321269999999,"d":"0.60"},{"v":4.692941289232492,"d":"4.69"},{"v":4.692941289232493,"d":"4.69"},{"v":1.8313814905,"d":"1.83"}]
["29101","Johnson","MO",{"v":0.783328465,"d":"0.78"},{"v":4.712553141162138,"d":"4.71"},{"v":4.712553141162138,"d":"4.71"},{"v":1.6485215595,"d":"1.65"}]
["29103","Knox","MO",{"v":0.868855932,"d":"0.87"},{"v":4.9381947910361585,"d":"4.94"},{"v":4.9381947910361585,"d":"4.94"},{"v":1.773558135,"d":"1.77"}]
["29105","Laclede","MO",{"v":0.7357674599999999,"d":"0.74"},{"v":4.858376102219147,"d":"4.86"},{"v":4.858376102219147,"d":"4.86"},{"v":1.8830927965,"d":"1.88"}]
["29107","Lafayette","MO",{"v":0.765332848,"d":"0.77"},{"v":4.842349572148192,"d":"4.84"},{"v":4.842349572148193,"d":"4.84"},{"v":1.6545506079999999,"d":"1.65"}]
["29109","Lawrence","MO",{"v":0.776276023,"d":"0.78"},{"v":4.637512255318793,"d":"4.64"},{"v":4.637512255318793,"d":"4.64"},{"v":1.6419534425,"d":"1.64"}]
["29111","Lewis","MO",{"v":0.863112713,"d":"0.86"},{"v":4.892509098409058,"d":"4.89"},{"v":4.892509098409057,"d":"4.89"},{"v":1.8059166085000002,"d":"1.81"}]
["29113","Lincoln","MO",{"v":0.7660551550000001,"d":"0.77"},{"v":5.044631863516624,"d":"5.04"},{"v":5.044631863516624,"d":"5.04"},{"v":1.8261007705,"d":"1.83"}]
["29115","Linn","MO",{"v":0.7900014159999998,"d":"0.79"},{"v":4.852357508527142,"d":"4.85"},{"v":4.852357508527142,"d":"4.85"},{"v":1.7115827904999996,"d":"1.71"}]
["29117","Livingston","MO",{"v":0.736259966,"d":"0.74"},{"v":4.839843928837168,"d":"4.84"},{"v":4.839843928837168,"d":"4.84"},{"v":1.6120389505000003,"d":"1.61"}]
["29119","Mcdonald","MO",{"v":0.7943598150000001,"d":"0.79"},{"v":4.9154075509100545,"d":"4.92"},{"v":4.9154075509100545,"d":"4.92"},{"v":2.0808771065,"d":"2.08"}]
["29121","Macon","MO",{"v":0.7902114659999999,"d":"0.79"},{"v":4.951129236509565,"d":"4.95"},{"v":4.951129236509566,"d":"4.95"},{"v":1.7237473795,"d":"1.72"}]
["29123","Madison","MO",{"v":0.713364147,"d":"0.71"},{"v":4.912993491912556,"d":"4.91"},{"v":4.912993491912555,"d":"4.91"},{"v":2.1546740984999997,"d":"2.15"}]
["29125","Maries","MO",{"v":0.8319851439999999,"d":"0.83"},{"v":4.968748767589762,"d":"4.97"},{"v":4.968748767589762,"d":"4.97"},{"v":1.989871914,"d":"1.99"}]
["29127","Marion","MO",{"v":0.692536512,"d":"0.69"},{"v":4.583935033887116,"d":"4.58"},{"v":4.583935033887116,"d":"4.58"},{"v":1.574329807,"d":"1.57"}]
["29129","Mercer","MO",{"v":0.8574718729999999,"d":"0.86"},{"v":5.038207311611574,"d":"5.04"},{"v":5.0382073116115755,"d":"5.04"},{"v":1.8184043044999998,"d":"1.82"}]
["29131","Miller","MO",{"v":0.745752105,"d":"0.75"},{"v":4.99632605511112,"d":"5.00"},{"v":4.99632605511112,"d":"5.00"},{"v":1.9664830610000001,"d":"1.97"}]
["29133","Mississippi","MO",{"v":0.763044334,"d":"0.76"},{"v":4.2757374141503455,"d":"4.28"},{"v":4.275737414150346,"d":"4.28"},{"v":1.5086142489999999,"d":"1.51"}]
["29135","Moniteau","MO",{"v":0.763866061,"d":"0.76"},{"v":4.654925552766323,"d":"4.65"},{"v":4.654925552766323,"d":"4.65"},{"v":1.6962892109999999,"d":"1.70"}]
["29137","Monroe","MO",{"v":0.8590117039999999,"d":"0.86"},{"v":4.913914503531843,"d":"4.91"},{"v":4.913914503531843,"d":"4.91"},{"v":1.7960359959999999,"d":"1.80"}]
["29139","Montgomery","MO",{"v":0.78947967,"d":"0.79"},{"v":4.952786321253541,"d":"4.95"},{"v":4.952786321253541,"d":"4.95"},{"v":1.8591421925,"d":"1.86"}]
["29141","Morgan","MO",{"v":0.8081784870000001,"d":"0.81"},{"v":5.008198375266039,"d":"5.01"},{"v":5.008198375266039,"d":"5.01"},{"v":2.0040372525,"d":"2.00"}]
["29143","New Madrid","MO",{"v":0.8157010689999998,"d":"0.82"},{"v":4.366868248089875,"d":"4.37"},{"v":4.366868248089875,"d":"4.37"},{"v":1.5449548699999998,"d":"1.54"}]
["29145","Newton","MO",{"v":0.755203594,"d":"0.76"},{"v":4.719480879309633,"d":"4.72"},{"v":4.719480879309634,"d":"4.72"},{"v":1.7546787270000002,"d":"1.75"}]
["29147","Nodaway","MO",{"v":0.752574205,"d":"0.75"},{"v":4.877944555674434,"d":"4.88"},{"v":4.877944555674434,"d":"4.88"},{"v":1.5972554884999999,"d":"1.60"}]
["29149","Oregon","MO",{"v":0.7557828900000001,"d":"0.76"},{"v":5.00217616004469,"d":"5.00"},{"v":5.002176160044691,"d":"5.00"},{"v":2.0946455395,"d":"2.09"}]
["29151","Osage","MO",{"v":0.8199061680000002,"d":"0.82"},{"v":5.10499296103151,"d":"5.10"},{"v":5.10499296103151,"d":"5.10"},{"v":2.008917167,"d":"2.01"}]
["29153","Ozark","MO",{"v":0.802406987,"d":"0.80"},{"v":4.997959724194199,"d":"5.00"},{"v":4.9979597241941995,"d":"5.00"},{"v":2.104815186,"d":"2.10"}]
["29155","Pemiscot","MO",{"v":0.802217435,"d":"0.80"},{"v":4.284102444990906,"d":"4.28"},{"v":4.284102444990907,"d":"4.28"},{"v":1.526545993,"d":"1.53"}]
["29157","Perry","MO",{"v":0.734283267,"d":"0.73"},{"v":4.679623452058726,"d":"4.68"},{"v":4.679623452058726,"d":"4.68"},{"v":1.797084108,"d":"1.80"}]
["29159","Pettis","MO",{"v":0.7371634900000001,"d":"0.74"},{"v":4.6154115271937,"d":"4.62"},{"v":4.6154115271937,"d":"4.62"},{"v":1.5662792505,"d":"1.57"}]
["29161","Phelps","MO",{"v":0.6830392390000001,"d":"0.68"},{"v":4.780394967641915,"d":"4.78"},{"v":4.780394967641915,"d":"4.78"},{"v":1.9850337190000005,"d":"1.99"}]
["29163","Pike","MO",{"v":0.7562686120000001,"d":"0.76"},{"v":4.901554436200382,"d":"4.90"},{"v":4.901554436200382,"d":"4.90"},{"v":1.7636323889999999,"d":"1.76"}]
["29165","Platte","MO",{"v":0.636404325,"d":"0.64"},{"v":4.71562362973244,"d":"4.72"},{"v":4.715623629732439,"d":"4.72"},{"v":1.5276506835,"d":"1.53"}]
["29167","Polk","MO",{"v":0.784947421,"d":"0.78"},{"v":4.863100522179957,"d":"4.86"},{"v":4.863100522179957,"d":"4.86"},{"v":1.7497509295,"d":"1.75"}]
["29169","Pulaski","MO",{"v":0.709095289,"d":"0.71"},{"v":4.8578508695279385,"d":"4.86"},{"v":4.8578508695279385,"d":"4.86"},{"v":2.0309501835000003,"d":"2.03"}]
["29171","Putnam","MO",{"v":0.859772541,"d":"0.86"},{"v":4.9519919781361725,"d":"4.95"},{"v":4.9519919781361725,"d":"4.95"},{"v":1.8504228965000002,"d":"1.85"}]
["29173","Ralls","MO",{"v":0.844004651,"d":"0.84"},{"v":4.999723469372154,"d":"5.00"},{"v":4.999723469372153,"d":"5.00"},{"v":1.8093203395000004,"d":"1.81"}]
["29175","Randolph","MO",{"v":0.7301490729999999,"d":"0.73"},{"v":4.7492313912830255,"d":"4.75"},{"v":4.749231391283025,"d":"4.75"},{"v":1.6856581375000002,"d":"1.69"}]
["29177","Ray","MO",{"v":0.79296989,"d":"0.79"},{"v":4.931203898731541,"d":"4.93"},{"v":4.931203898731541,"d":"4.93"},{"v":1.7518393374999999,"d":"1.75"}]
["29179","Reynolds","MO",{"v":0.7672907580000001,"d":"0.77"},{"v":5.138842678206288,"d":"5.14"},{"v":5.138842678206288,"d":"5.14"},{"v":2.3514933399999998,"d":"2.35"}]
["29181","Ripley","MO",{"v":0.777210479,"d":"0.78"},{"v":5.017887284414918,"d":"5.02"},{"v":5.017887284414918,"d":"5.02"},{"v":2.216135234,"d":"2.22"}]
["29183","St Charles","MO",{"v":0.538394424,"d":"0.54"},{"v":4.288327945472906,"d":"4.29"},{"v":4.288327945472906,"d":"4.29"},{"v":1.4501779805000001,"d":"1.45"}]
["29185","St Clair","MO",{"v":0.834029615,"d":"0.83"},{"v":5.036811052812367,"d":"5.04"},{"v":5.036811052812367,"d":"5.04"},{"v":1.934055756,"d":"1.93"}]
["29186","Ste Genevieve","MO",{"v":0.7538653110000001,"d":"0.75"},{"v":4.8767032700782345,"d":"4.88"},{"v":4.876703270078235,"d":"4.88"},{"v":2.0029921405,"d":"2.00"}]
["29187","St Francois","MO",{"v":0.656372818,"d":"0.66"},{"v":4.806834397878146,"d":"4.81"},{"v":4.806834397878147,"d":"4.81"},{"v":1.8869178155000002,"d":"1.89"}]
["29189","St Louis","MO",{"v":0.340563179,"d":"0.34"},{"v":0.22940876176029665,"d":"0.23"},{"v":0.22940876176029665,"d":"0.23"},{"v":1.3109163625000002,"d":"1.31"}]
["29195","Saline","MO",{"v":0.7508268370000001,"d":"0.75"},{"v":4.762171342675351,"d":"4.76"},{"v":4.762171342675352,"d":"4.76"},{"v":1.6327782985000001,"d":"1.63"}]
["29197","Schuyler","MO",{"v":0.8748464630000001,"d":"0.87"},{"v":4.929797106732267,"d":"4.93"},{"v":4.929797106732268,"d":"4.93"},{"v":1.7984873920000002,"d":"1.80"}]
["29199","Scotland","MO",{"v":0.873584092,"d":"0.87"},{"v":4.82493880409755,"d":"4.82"},{"v":4.824938804097551,"d":"4.82"},{"v":1.7762045884999997,"d":"1.78"}]
["29201","Scott","MO",{"v":0.7531887949999999,"d":"0.75"},{"v":4.466847523365301,"d":"4.47"},{"v":4.466847523365301,"d":"4.47"},{"v":1.5055029740000003,"d":"1.51"}]
["29203","Shannon","MO",{"v":0.768954265,"d":"0.77"},{"v":5.133900689677432,"d":"5.13"},{"v":5.133900689677432,"d":"5.13"},{"v":2.343711081,"d":"2.34"}]
["29205","Shelby","MO",{"v":0.883883524,"d":"0.88"},{"v":4.970741021216323,"d":"4.97"},{"v":4.970741021216323,"d":"4.97"},{"v":1.7733409640000002,"d":"1.77"}]
["29207","Stoddard","MO",{"v":0.831521827,"d":"0.83"},{"v":4.4610188369690285,"d":"4.46"},{"v":4.4610188369690285,"d":"4.46"},{"v":1.627698001,"d":"1.63"}]
["29209","Stone","MO",{"v":0.7704622020000002,"d":"0.77"},{"v":4.939081289969329,"d":"4.94"},{"v":4.939081289969329,"d":"4.94"},{"v":1.9770880064999996,"d":"1.98"}]
["29211","Sullivan","MO",{"v":0.855482284,"d":"0.86"},{"v":4.973712104707907,"d":"4.97"},{"v":4.973712104707906,"d":"4.97"},{"v":1.836153479,"d":"1.84"}]
["29213","Taney","MO",{"v":0.6341952329999999,"d":"0.63"},{"v":5.014734650007651,"d":"5.01"},{"v":5.01473465000765,"d":"5.01"},{"v":1.9565732315000002,"d":"1.96"}]
["29215","Texas","MO",{"v":0.803626355,"d":"0.80"},{"v":5.019043459130436,"d":"5.02"},{"v":5.019043459130437,"d":"5.02"},{"v":2.085734103,"d":"2.09"}]
["29217","Vernon","MO",{"v":0.778372602,"d":"0.78"},{"v":4.759444743060459,"d":"4.76"},{"v":4.75944474306046,"d":"4.76"},{"v":1.6748191534999999,"d":"1.67"}]
["29219","Warren","MO",{"v":0.726012191,"d":"0.73"},{"v":5.104861807807849,"d":"5.10"},{"v":5.104861807807849,"d":"5.10"},{"v":1.9150435175000002,"d":"1.92"}]
["29221","Washington","MO",{"v":0.7264742820000001,"d":"0.73"},{"v":5.098388066910357,"d":"5.10"},{"v":5.098388066910357,"d":"5.10"},{"v":2.2104237455,"d":"2.21"}]
["29223","Wayne","MO",{"v":0.76077757,"d":"0.76"},{"v":5.113504429438172,"d":"5.11"},{"v":5.113504429438173,"d":"5.11"},{"v":2.3346875624999996,"d":"2.33"}]
["29225","Webster","MO",{"v":0.7733653130000001,"d":"0.77"},{"v":4.784344861114656,"d":"4.78"},{"v":4.784344861114656,"d":"4.78"},{"v":1.8300111305000002,"d":"1.83"}]
["29227","Worth","MO",{"v":0.8607405199999999,"d":"0.86"},{"v":4.979927353116221,"d":"4.98"},{"v":4.9799273531162225,"d":"4.98"},{"v":1.7915711914999999,"d":"1.79"}]
["29229","Wright","MO",{"v":0.782743935,"d":"0.78"},{"v":4.795043202737803,"d":"4.80"},{"v":4.795043202737803,"d":"4.80"},{"v":1.8914177005,"d":"1.89"}]
["29510","St Louis City","MO",{"v":0.127309491,"d":"0.13"},{"v":9.15602518228005e-08,"d":"0.00"},{"v":9.1560251822800517E-8,"d":"0.00"},{"v":0.9064369724999999,"d":"0.91"}]
["30001","Beaverhead","MT",{"v":0.24313106199999998,"d":"0.24"},{"v":2.026611531510722,"d":"2.03"},{"v":2.0266115315107225,"d":"2.03"},{"v":0.6664391195,"d":"0.67"}]
["30003","Big Horn","MT",{"v":0.263785233,"d":"0.26"},{"v":1.9613349716121014,"d":"1.96"},{"v":1.9613349716121014,"d":"1.96"},{"v":0.63703892,"d":"0.64"}]
["30005","Blaine","MT",{"v":0.290256984,"d":"0.29"},{"v":2.0062947117580254,"d":"2.01"},{"v":2.0062947117580254,"d":"2.01"},{"v":0.6707890365,"d":"0.67"}]
["30007","Broadwater","MT",{"v":0.282777815,"d":"0.28"},{"v":2.0269256199585026,"d":"2.03"},{"v":2.0269256199585026,"d":"2.03"},{"v":0.6944597570000001,"d":"0.69"}]
["30009","Carbon","MT",{"v":0.292376892,"d":"0.29"},{"v":1.9347095883542247,"d":"1.93"},{"v":1.9347095883542247,"d":"1.93"},{"v":0.6708653459999999,"d":"0.67"}]
["30011","Carter","MT",{"v":0.2900271529999999,"d":"0.29"},{"v":2.0042448358199074,"d":"2.00"},{"v":2.0042448358199074,"d":"2.00"},{"v":0.6609173644999999,"d":"0.66"}]
["30013","Cascade","MT",{"v":0.23079952399999998,"d":"0.23"},{"v":1.8883568334109502,"d":"1.89"},{"v":1.8883568334109504,"d":"1.89"},{"v":0.573553937,"d":"0.57"}]
["30015","Chouteau","MT",{"v":0.28970463999999996,"d":"0.29"},{"v":2.0146784119793733,"d":"2.01"},{"v":2.0146784119793733,"d":"2.01"},{"v":0.665961704,"d":"0.67"}]
["30017","Custer","MT",{"v":0.23481873900000003,"d":"0.23"},{"v":1.9028525470428388,"d":"1.90"},{"v":1.9028525470428388,"d":"1.90"},{"v":0.553318579,"d":"0.55"}]
["30019","Daniels","MT",{"v":0.28733935799999993,"d":"0.29"},{"v":2.053366238260841,"d":"2.05"},{"v":2.053366238260841,"d":"2.05"},{"v":0.6672528780000001,"d":"0.67"}]
["30021","Dawson","MT",{"v":0.236388672,"d":"0.24"},{"v":1.9443076561796637,"d":"1.94"},{"v":1.9443076561796637,"d":"1.94"},{"v":0.5869198480000001,"d":"0.59"}]
["30023","Deer Lodge","MT",{"v":0.227036804,"d":"0.23"},{"v":1.9490137015434892,"d":"1.95"},{"v":1.9490137015434892,"d":"1.95"},{"v":0.6542339140000001,"d":"0.65"}]
["30025","Fallon","MT",{"v":0.29456357,"d":"0.29"},{"v":1.964244889497293,"d":"1.96"},{"v":1.964244889497293,"d":"1.96"},{"v":0.6587446519999999,"d":"0.66"}]
["30027","Fergus","MT",{"v":0.24716990399999997,"d":"0.25"},{"v":1.9520767389844849,"d":"1.95"},{"v":1.9520767389844846,"d":"1.95"},{"v":0.6129026000000001,"d":"0.61"}]
["30029","Flathead","MT",{"v":0.23147720399999996,"d":"0.23"},{"v":2.0335638329994508,"d":"2.03"},{"v":2.0335638329994508,"d":"2.03"},{"v":0.7572307605,"d":"0.76"}]
["30031","Gallatin","MT",{"v":0.23617447600000002,"d":"0.24"},{"v":1.9975094928495227,"d":"2.00"},{"v":1.9975094928495227,"d":"2.00"},{"v":0.652247559,"d":"0.65"}]
["30033","Garfield","MT",{"v":0.287772944,"d":"0.29"},{"v":2.052721328883215,"d":"2.05"},{"v":2.0527213288832153,"d":"2.05"},{"v":0.6766642169999999,"d":"0.68"}]
["30035","Glacier","MT",{"v":0.24319878399999997,"d":"0.24"},{"v":2.0011901557995535,"d":"2.00"},{"v":2.0011901557995535,"d":"2.00"},{"v":0.6284286705000001,"d":"0.63"}]
["30037","Golden Valley","MT",{"v":0.291838069,"d":"0.29"},{"v":2.014022028943011,"d":"2.01"},{"v":2.0140220289430113,"d":"2.01"},{"v":0.6663387614999999,"d":"0.67"}]
["30039","Granite","MT",{"v":0.270007635,"d":"0.27"},{"v":2.0656863795349656,"d":"2.07"},{"v":2.0656863795349656,"d":"2.07"},{"v":0.768911229,"d":"0.77"}]
["30041","Hill","MT",{"v":0.24390141199999998,"d":"0.24"},{"v":1.9417816477218517,"d":"1.94"},{"v":1.941781647721852,"d":"1.94"},{"v":0.593668242,"d":"0.59"}]
["30043","Jefferson","MT",{"v":0.272324234,"d":"0.27"},{"v":2.0614771853174645,"d":"2.06"},{"v":2.061477185317465,"d":"2.06"},{"v":0.7497480639999998,"d":"0.75"}]
["30045","Judith Basin","MT",{"v":0.283934448,"d":"0.28"},{"v":2.031977609330346,"d":"2.03"},{"v":2.031977609330346,"d":"2.03"},{"v":0.6938532055,"d":"0.69"}]
["30047","Lake","MT",{"v":0.259128506,"d":"0.26"},{"v":2.0585024693627254,"d":"2.06"},{"v":2.058502469362726,"d":"2.06"},{"v":0.7344171129999998,"d":"0.73"}]
["30049","Lewis and Clark","MT",{"v":0.231269636,"d":"0.23"},{"v":1.9305734770799758,"d":"1.93"},{"v":1.9305734770799758,"d":"1.93"},{"v":0.6432754725,"d":"0.64"}]
["30051","Liberty","MT",{"v":0.276519836,"d":"0.28"},{"v":1.9805326298225474,"d":"1.98"},{"v":1.9805326298225476,"d":"1.98"},{"v":0.664556968,"d":"0.66"}]
["30053","Lincoln","MT",{"v":0.239366876,"d":"0.24"},{"v":2.157069140684609,"d":"2.16"},{"v":2.157069140684609,"d":"2.16"},{"v":0.8549203474999999,"d":"0.85"}]
["30055","McCone","MT",{"v":0.29145089999999996,"d":"0.29"},{"v":2.0468313324309713,"d":"2.05"},{"v":2.0468313324309713,"d":"2.05"},{"v":0.6696788140000001,"d":"0.67"}]
["30057","Madison","MT",{"v":0.274572194,"d":"0.27"},{"v":2.070706109457567,"d":"2.07"},{"v":2.0707061094575665,"d":"2.07"},{"v":0.711939224,"d":"0.71"}]
["30059","Meagher","MT",{"v":0.280446778,"d":"0.28"},{"v":2.0495778442726027,"d":"2.05"},{"v":2.049577844272603,"d":"2.05"},{"v":0.7181387249999999,"d":"0.72"}]
["30061","Mineral","MT",{"v":0.257039485,"d":"0.26"},{"v":2.1592451219715763,"d":"2.16"},{"v":2.1592451219715763,"d":"2.16"},{"v":0.8352594189999999,"d":"0.84"}]
["30063","Missoula","MT",{"v":0.213145413,"d":"0.21"},{"v":1.9465419919155889,"d":"1.95"},{"v":1.946541991915589,"d":"1.95"},{"v":0.681866644,"d":"0.68"}]
["30065","Musselshell","MT",{"v":0.291845531,"d":"0.29"},{"v":2.0043253790313655,"d":"2.00"},{"v":2.0043253790313655,"d":"2.00"},{"v":0.6716454425000001,"d":"0.67"}]
["30067","Park","MT",{"v":0.24732365300000003,"d":"0.25"},{"v":1.966073671105999,"d":"1.97"},{"v":1.966073671105999,"d":"1.97"},{"v":0.6560818749999999,"d":"0.66"}]
["30069","Petroleum","MT",{"v":0.290447842,"d":"0.29"},{"v":2.0113609619579402,"d":"2.01"},{"v":2.01136096195794,"d":"2.01"},{"v":0.663726422,"d":"0.66"}]
["30071","Phillips","MT",{"v":0.286364791,"d":"0.29"},{"v":1.9865068888756336,"d":"1.99"},{"v":1.986506888875634,"d":"1.99"},{"v":0.6689223285000002,"d":"0.67"}]
["30073","Pondera","MT",{"v":0.250465481,"d":"0.25"},{"v":1.9846521338772425,"d":"1.98"},{"v":1.9846521338772425,"d":"1.98"},{"v":0.6260089185,"d":"0.63"}]
["30075","Powder River","MT",{"v":0.28940296599999993,"d":"0.29"},{"v":2.0223992058885205,"d":"2.02"},{"v":2.0223992058885205,"d":"2.02"},{"v":0.6763692765,"d":"0.68"}]
["30077","Powell","MT",{"v":0.23175326100000002,"d":"0.23"},{"v":1.9856451647409268,"d":"1.99"},{"v":1.9856451647409268,"d":"1.99"},{"v":0.695371201,"d":"0.70"}]
["30079","Prairie","MT",{"v":0.2927798670000001,"d":"0.29"},{"v":1.9739412030026686,"d":"1.97"},{"v":1.9739412030026684,"d":"1.97"},{"v":0.6529886715000001,"d":"0.65"}]
["30081","Ravalli","MT",{"v":0.2634528199999999,"d":"0.26"},{"v":2.0069654702913815,"d":"2.01"},{"v":2.0069654702913815,"d":"2.01"},{"v":0.7241299185000001,"d":"0.72"}]
["30083","Richland","MT",{"v":0.24587839900000003,"d":"0.25"},{"v":2.004722409258896,"d":"2.00"},{"v":2.004722409258896,"d":"2.00"},{"v":0.6061370090000001,"d":"0.61"}]
["30085","Roosevelt","MT",{"v":0.248023257,"d":"0.25"},{"v":1.9907427335925794,"d":"1.99"},{"v":1.9907427335925794,"d":"1.99"},{"v":0.6059964809999999,"d":"0.61"}]
["30087","Rosebud","MT",{"v":0.2947288699999999,"d":"0.29"},{"v":1.988440434468748,"d":"1.99"},{"v":1.9884404344687479,"d":"1.99"},{"v":0.6677190894999999,"d":"0.67"}]
["30089","Sanders","MT",{"v":0.26404061100000004,"d":"0.26"},{"v":2.1139336743683717,"d":"2.11"},{"v":2.113933674368371,"d":"2.11"},{"v":0.802881508,"d":"0.80"}]
["30091","Sheridan","MT",{"v":0.289053651,"d":"0.29"},{"v":2.0481579537729457,"d":"2.05"},{"v":2.0481579537729453,"d":"2.05"},{"v":0.6643764930000001,"d":"0.66"}]
["30093","Silver Bow","MT",{"v":0.209848914,"d":"0.21"},{"v":1.9453438175826792,"d":"1.95"},{"v":1.9453438175826794,"d":"1.95"},{"v":0.6170532155,"d":"0.62"}]
["30095","Stillwater","MT",{"v":0.29129927,"d":"0.29"},{"v":1.951435162086214,"d":"1.95"},{"v":1.9514351620862143,"d":"1.95"},{"v":0.6684534945000001,"d":"0.67"}]
["30097","Sweet Grass","MT",{"v":0.289874647,"d":"0.29"},{"v":1.9567908483186072,"d":"1.96"},{"v":1.9567908483186072,"d":"1.96"},{"v":0.6837599230000001,"d":"0.68"}]
["30099","Teton","MT",{"v":0.283199813,"d":"0.28"},{"v":2.017929009163199,"d":"2.02"},{"v":2.017929009163199,"d":"2.02"},{"v":0.681560013,"d":"0.68"}]
["30101","Toole","MT",{"v":0.24977884299999997,"d":"0.25"},{"v":1.9826876921127112,"d":"1.98"},{"v":1.9826876921127112,"d":"1.98"},{"v":0.5990168724999999,"d":"0.60"}]
["30103","Treasure","MT",{"v":0.291955921,"d":"0.29"},{"v":2.0101065201697574,"d":"2.01"},{"v":2.0101065201697574,"d":"2.01"},{"v":0.6633210774999999,"d":"0.66"}]
["30105","Valley","MT",{"v":0.2699501369999999,"d":"0.27"},{"v":1.9622296914400479,"d":"1.96"},{"v":1.9622296914400479,"d":"1.96"},{"v":0.6190872105,"d":"0.62"}]
["30107","Wheatland","MT",{"v":0.291060244,"d":"0.29"},{"v":1.9585287872789836,"d":"1.96"},{"v":1.9585287872789838,"d":"1.96"},{"v":0.6639454574999998,"d":"0.66"}]
["30109","Wibaux","MT",{"v":0.29499407799999994,"d":"0.29"},{"v":1.949977660145852,"d":"1.95"},{"v":1.9499776601458523,"d":"1.95"},{"v":0.6552278504999999,"d":"0.66"}]
["30111","Yellowstone","MT",{"v":0.232244059,"d":"0.23"},{"v":1.8549340333037354,"d":"1.85"},{"v":1.8549340333037354,"d":"1.85"},{"v":0.5447821975,"d":"0.54"}]
["31001","Adams","NE",{"v":0.22727839,"d":"0.23"},{"v":1.534322189042425,"d":"1.53"},{"v":1.5343221890424248,"d":"1.53"},{"v":0.4696451589999999,"d":"0.47"}]
["31003","Antelope","NE",{"v":0.269816161,"d":"0.27"},{"v":1.6712347164400045,"d":"1.67"},{"v":1.6712347164400048,"d":"1.67"},{"v":0.5706847389999999,"d":"0.57"}]
["31005","Arthur","NE",{"v":0.279072297,"d":"0.28"},{"v":1.7161078668350387,"d":"1.72"},{"v":1.7161078668350385,"d":"1.72"},{"v":0.5606689399999999,"d":"0.56"}]
["31007","Banner","NE",{"v":0.277767372,"d":"0.28"},{"v":1.6978566850927597,"d":"1.70"},{"v":1.6978566850927597,"d":"1.70"},{"v":0.5596732935000001,"d":"0.56"}]
["31009","Blaine","NE",{"v":0.272111655,"d":"0.27"},{"v":1.7142222808781962,"d":"1.71"},{"v":1.7142222808781962,"d":"1.71"},{"v":0.5643511775,"d":"0.56"}]
["31011","Boone","NE",{"v":0.271562378,"d":"0.27"},{"v":1.6785543998919352,"d":"1.68"},{"v":1.6785543998919354,"d":"1.68"},{"v":0.5682574880000001,"d":"0.57"}]
["31013","Box Butte","NE",{"v":0.221399381,"d":"0.22"},{"v":1.6149634356201874,"d":"1.61"},{"v":1.6149634356201874,"d":"1.61"},{"v":0.4803669945,"d":"0.48"}]
["31015","Boyd","NE",{"v":0.269441918,"d":"0.27"},{"v":1.7233302151188203,"d":"1.72"},{"v":1.7233302151188201,"d":"1.72"},{"v":0.5759393125000001,"d":"0.58"}]
["31017","Brown","NE",{"v":0.272775811,"d":"0.27"},{"v":1.643540383182142,"d":"1.64"},{"v":1.643540383182142,"d":"1.64"},{"v":0.572145488,"d":"0.57"}]
["31019","Buffalo","NE",{"v":0.22765240200000003,"d":"0.23"},{"v":1.5954551141542326,"d":"1.60"},{"v":1.5954551141542326,"d":"1.60"},{"v":0.4924869635,"d":"0.49"}]
["31021","Burt","NE",{"v":0.273395095,"d":"0.27"},{"v":1.669924686063269,"d":"1.67"},{"v":1.669924686063269,"d":"1.67"},{"v":0.5713339119999999,"d":"0.57"}]
["31023","Butler","NE",{"v":0.252835182,"d":"0.25"},{"v":1.6372112458034926,"d":"1.64"},{"v":1.6372112458034924,"d":"1.64"},{"v":0.5358464339999999,"d":"0.54"}]
["31025","Cass","NE",{"v":0.25303267,"d":"0.25"},{"v":1.6210642408683102,"d":"1.62"},{"v":1.6210642408683098,"d":"1.62"},{"v":0.544435538,"d":"0.54"}]
["31027","Cedar","NE",{"v":0.271767735,"d":"0.27"},{"v":1.6738666376931968,"d":"1.67"},{"v":1.673866637693197,"d":"1.67"},{"v":0.5693595585,"d":"0.57"}]
["31029","Chase","NE",{"v":0.279686585,"d":"0.28"},{"v":1.615404196225972,"d":"1.62"},{"v":1.615404196225972,"d":"1.62"},{"v":0.5495809990000001,"d":"0.55"}]
["31031","Cherry","NE",{"v":0.23944870099999999,"d":"0.24"},{"v":1.6816776516394376,"d":"1.68"},{"v":1.6816776516394376,"d":"1.68"},{"v":0.5217031849999999,"d":"0.52"}]
["31033","Cheyenne","NE",{"v":0.233805811,"d":"0.23"},{"v":1.5732616605219338,"d":"1.57"},{"v":1.5732616605219338,"d":"1.57"},{"v":0.4994405364999999,"d":"0.50"}]
["31035","Clay","NE",{"v":0.284267753,"d":"0.28"},{"v":1.5637120561654887,"d":"1.56"},{"v":1.5637120561654887,"d":"1.56"},{"v":0.550149228,"d":"0.55"}]
["31037","Colfax","NE",{"v":0.239515538,"d":"0.24"},{"v":1.6423964643006013,"d":"1.64"},{"v":1.6423964643006013,"d":"1.64"},{"v":0.5165869465,"d":"0.52"}]
["31039","Cuming","NE",{"v":0.245046775,"d":"0.25"},{"v":1.6597617872957162,"d":"1.66"},{"v":1.6597617872957164,"d":"1.66"},{"v":0.5388639430000001,"d":"0.54"}]
["31041","Custer","NE",{"v":0.252536222,"d":"0.25"},{"v":1.6428860644221883,"d":"1.64"},{"v":1.6428860644221888,"d":"1.64"},{"v":0.5335808765,"d":"0.53"}]
["31043","Dakota","NE",{"v":0.20946719599999997,"d":"0.21"},{"v":1.654590634963534,"d":"1.65"},{"v":1.6545906349635342,"d":"1.65"},{"v":0.49634218300000005,"d":"0.50"}]
["31045","Dawes","NE",{"v":0.233134661,"d":"0.23"},{"v":1.6153591123117785,"d":"1.62"},{"v":1.6153591123117783,"d":"1.62"},{"v":0.516384755,"d":"0.52"}]
["31047","Dawson","NE",{"v":0.226088382,"d":"0.23"},{"v":1.630479482299612,"d":"1.63"},{"v":1.6304794822996123,"d":"1.63"},{"v":0.48785732200000004,"d":"0.49"}]
["31049","Deuel","NE",{"v":0.276871441,"d":"0.28"},{"v":1.5948047869248436,"d":"1.59"},{"v":1.5948047869248434,"d":"1.59"},{"v":0.5575194245,"d":"0.56"}]
["31051","Dixon","NE",{"v":0.268310972,"d":"0.27"},{"v":1.6802130517007967,"d":"1.68"},{"v":1.6802130517007967,"d":"1.68"},{"v":0.5779405435000001,"d":"0.58"}]
["31053","Dodge","NE",{"v":0.22330564899999997,"d":"0.22"},{"v":1.583028723932378,"d":"1.58"},{"v":1.5830287239323781,"d":"1.58"},{"v":0.48396822449999993,"d":"0.48"}]
["31055","Douglas","NE",{"v":0.11895785,"d":"0.12"},{"v":0.2764886414461195,"d":"0.28"},{"v":0.2764886414461195,"d":"0.28"},{"v":0.3893735009999999,"d":"0.39"}]
["31057","Dundy","NE",{"v":0.279465129,"d":"0.28"},{"v":1.5987757138788026,"d":"1.60"},{"v":1.5987757138788028,"d":"1.60"},{"v":0.5508959825,"d":"0.55"}]
["31059","Fillmore","NE",{"v":0.27830941500000006,"d":"0.28"},{"v":1.5749266409278615,"d":"1.57"},{"v":1.5749266409278613,"d":"1.57"},{"v":0.5491890545000001,"d":"0.55"}]
["31061","Franklin","NE",{"v":0.280305087,"d":"0.28"},{"v":1.5721699124394015,"d":"1.57"},{"v":1.5721699124394015,"d":"1.57"},{"v":0.552178467,"d":"0.55"}]
["31063","Frontier","NE",{"v":0.279209502,"d":"0.28"},{"v":1.6302873817266332,"d":"1.63"},{"v":1.630287381726633,"d":"1.63"},{"v":0.5534355099999999,"d":"0.55"}]
["31065","Furnas","NE",{"v":0.281447273,"d":"0.28"},{"v":1.5730606947481518,"d":"1.57"},{"v":1.5730606947481516,"d":"1.57"},{"v":0.5491620155,"d":"0.55"}]
["31067","Gage","NE",{"v":0.237287351,"d":"0.24"},{"v":1.561314907613878,"d":"1.56"},{"v":1.561314907613878,"d":"1.56"},{"v":0.5057368160000001,"d":"0.51"}]
["31069","Garden","NE",{"v":0.27845375,"d":"0.28"},{"v":1.6514380090887355,"d":"1.65"},{"v":1.6514380090887353,"d":"1.65"},{"v":0.557609889,"d":"0.56"}]
["31071","Garfield","NE",{"v":0.269310277,"d":"0.27"},{"v":1.668804514139878,"d":"1.67"},{"v":1.668804514139878,"d":"1.67"},{"v":0.567782862,"d":"0.57"}]
["31073","Gosper","NE",{"v":0.27931858200000004,"d":"0.28"},{"v":1.6090048107960122,"d":"1.61"},{"v":1.6090048107960122,"d":"1.61"},{"v":0.5526564635000001,"d":"0.55"}]
["31075","Grant","NE",{"v":0.273253259,"d":"0.27"},{"v":1.7218260187456425,"d":"1.72"},{"v":1.7218260187456425,"d":"1.72"},{"v":0.5661505030000001,"d":"0.57"}]
["31077","Greeley","NE",{"v":0.277651416,"d":"0.28"},{"v":1.651582783509423,"d":"1.65"},{"v":1.651582783509423,"d":"1.65"},{"v":0.5584441469999999,"d":"0.56"}]
["31079","Hall","NE",{"v":0.21585776300000004,"d":"0.22"},{"v":1.5563975975265336,"d":"1.56"},{"v":1.5563975975265336,"d":"1.56"},{"v":0.4638543255,"d":"0.46"}]
["31081","Hamilton","NE",{"v":0.241797538,"d":"0.24"},{"v":1.5867689648179921,"d":"1.59"},{"v":1.586768964817992,"d":"1.59"},{"v":0.514971736,"d":"0.51"}]
["31083","Harlan","NE",{"v":0.277326224,"d":"0.28"},{"v":1.6026526324039574,"d":"1.60"},{"v":1.6026526324039574,"d":"1.60"},{"v":0.5568211735,"d":"0.56"}]
["31085","Hayes","NE",{"v":0.28071039500000006,"d":"0.28"},{"v":1.6605858478403634,"d":"1.66"},{"v":1.6605858478403634,"d":"1.66"},{"v":0.54937514,"d":"0.55"}]
["31087","Hitchcock","NE",{"v":0.27779169800000003,"d":"0.28"},{"v":1.6585376279656876,"d":"1.66"},{"v":1.658537627965688,"d":"1.66"},{"v":0.5539958494999999,"d":"0.55"}]
["31089","Holt","NE",{"v":0.24823043399999994,"d":"0.25"},{"v":1.6611518196878658,"d":"1.66"},{"v":1.6611518196878658,"d":"1.66"},{"v":0.5358265945,"d":"0.54"}]
["31091","Hooker","NE",{"v":0.27633300099999997,"d":"0.28"},{"v":1.7099226688715317,"d":"1.71"},{"v":1.7099226688715312,"d":"1.71"},{"v":0.5656417955,"d":"0.57"}]
["31093","Howard","NE",{"v":0.274119751,"d":"0.27"},{"v":1.6608567210835454,"d":"1.66"},{"v":1.6608567210835454,"d":"1.66"},{"v":0.561621138,"d":"0.56"}]
["31095","Jefferson","NE",{"v":0.239129498,"d":"0.24"},{"v":1.595158861538282,"d":"1.60"},{"v":1.5951588615382817,"d":"1.60"},{"v":0.510485021,"d":"0.51"}]
["31097","Johnson","NE",{"v":0.275340329,"d":"0.28"},{"v":1.6100189643154739,"d":"1.61"},{"v":1.6100189643154739,"d":"1.61"},{"v":0.5629166215,"d":"0.56"}]
["31099","Kearney","NE",{"v":0.24636409499999995,"d":"0.25"},{"v":1.5595863431223118,"d":"1.56"},{"v":1.5595863431223118,"d":"1.56"},{"v":0.509144351,"d":"0.51"}]
["31101","Keith","NE",{"v":0.24407054799999994,"d":"0.24"},{"v":1.6098361649994535,"d":"1.61"},{"v":1.609836164999453,"d":"1.61"},{"v":0.507290203,"d":"0.51"}]
["31103","Keya Paha","NE",{"v":0.269433448,"d":"0.27"},{"v":1.7092664662406725,"d":"1.71"},{"v":1.7092664662406722,"d":"1.71"},{"v":0.5798846544999999,"d":"0.58"}]
["31105","Kimball","NE",{"v":0.27632620599999996,"d":"0.28"},{"v":1.5916687619618486,"d":"1.59"},{"v":1.5916687619618486,"d":"1.59"},{"v":0.5595468835,"d":"0.56"}]
["31107","Knox","NE",{"v":0.27147115,"d":"0.27"},{"v":1.7016906411929567,"d":"1.70"},{"v":1.7016906411929569,"d":"1.70"},{"v":0.5765532134999999,"d":"0.58"}]
["31109","Lancaster","NE",{"v":0.187653386,"d":"0.19"},{"v":1.5279735273352113,"d":"1.53"},{"v":1.5279735273352113,"d":"1.53"},{"v":0.44562819549999994,"d":"0.45"}]
["31111","Lincoln","NE",{"v":0.229341808,"d":"0.23"},{"v":1.5721730130883573,"d":"1.57"},{"v":1.572173013088357,"d":"1.57"},{"v":0.48342103950000004,"d":"0.48"}]
["31113","Logan","NE",{"v":0.273605907,"d":"0.27"},{"v":1.7147656624298537,"d":"1.71"},{"v":1.7147656624298537,"d":"1.71"},{"v":0.5641909555000001,"d":"0.56"}]
["31115","Loup","NE",{"v":0.272206679,"d":"0.27"},{"v":1.7269236533305554,"d":"1.73"},{"v":1.7269236533305554,"d":"1.73"},{"v":0.569694875,"d":"0.57"}]
["31117","McPherson","NE",{"v":0.275674817,"d":"0.28"},{"v":1.6910056156756341,"d":"1.69"},{"v":1.6910056156756343,"d":"1.69"},{"v":0.5656300034999999,"d":"0.57"}]
["31119","Madison","NE",{"v":0.217765769,"d":"0.22"},{"v":1.6278961967165895,"d":"1.63"},{"v":1.6278961967165895,"d":"1.63"},{"v":0.49378248049999995,"d":"0.49"}]
["31121","Merrick","NE",{"v":0.24443687799999997,"d":"0.24"},{"v":1.6195697766769244,"d":"1.62"},{"v":1.6195697766769246,"d":"1.62"},{"v":0.524661833,"d":"0.52"}]
["31123","Morrill","NE",{"v":0.276124554,"d":"0.28"},{"v":1.6394260608323625,"d":"1.64"},{"v":1.6394260608323625,"d":"1.64"},{"v":0.5586794375,"d":"0.56"}]
["31125","Nance","NE",{"v":0.274346083,"d":"0.27"},{"v":1.6279259370497583,"d":"1.63"},{"v":1.6279259370497579,"d":"1.63"},{"v":0.5665546450000001,"d":"0.57"}]
["31127","Nemaha","NE",{"v":0.239775845,"d":"0.24"},{"v":1.5922451152936745,"d":"1.59"},{"v":1.5922451152936745,"d":"1.59"},{"v":0.516228842,"d":"0.52"}]
["31129","Nuckolls","NE",{"v":0.27753058300000005,"d":"0.28"},{"v":1.569312155164624,"d":"1.57"},{"v":1.5693121551646243,"d":"1.57"},{"v":0.552625327,"d":"0.55"}]
["31131","Otoe","NE",{"v":0.24519444500000004,"d":"0.25"},{"v":1.563946103816739,"d":"1.56"},{"v":1.5639461038167388,"d":"1.56"},{"v":0.520989994,"d":"0.52"}]
["31133","Pawnee","NE",{"v":0.274772029,"d":"0.27"},{"v":1.618824755506062,"d":"1.62"},{"v":1.6188247555060618,"d":"1.62"},{"v":0.565266033,"d":"0.57"}]
["31135","Perkins","NE",{"v":0.280034713,"d":"0.28"},{"v":1.6028469612979754,"d":"1.60"},{"v":1.6028469612979754,"d":"1.60"},{"v":0.548464706,"d":"0.55"}]
["31137","Phelps","NE",{"v":0.236508063,"d":"0.24"},{"v":1.5466948643040408,"d":"1.55"},{"v":1.5466948643040408,"d":"1.55"},{"v":0.495260163,"d":"0.50"}]
["31139","Pierce","NE",{"v":0.272715599,"d":"0.27"},{"v":1.673815586585793,"d":"1.67"},{"v":1.673815586585793,"d":"1.67"},{"v":0.5696838735,"d":"0.57"}]
["31141","Platte","NE",{"v":0.22558591000000003,"d":"0.23"},{"v":1.6088178547144651,"d":"1.61"},{"v":1.6088178547144651,"d":"1.61"},{"v":0.49095234050000003,"d":"0.49"}]
["31143","Polk","NE",{"v":0.275302739,"d":"0.28"},{"v":1.632459007793647,"d":"1.63"},{"v":1.632459007793647,"d":"1.63"},{"v":0.5591703435,"d":"0.56"}]
["31145","Red Willow","NE",{"v":0.22971992099999994,"d":"0.23"},{"v":1.5607081577280586,"d":"1.56"},{"v":1.5607081577280584,"d":"1.56"},{"v":0.4829260965000001,"d":"0.48"}]
["31147","Richardson","NE",{"v":0.241718012,"d":"0.24"},{"v":1.5743695615250937,"d":"1.57"},{"v":1.5743695615250937,"d":"1.57"},{"v":0.5175229179999999,"d":"0.52"}]
["31149","Rock","NE",{"v":0.275995919,"d":"0.28"},{"v":1.6758983863138937,"d":"1.68"},{"v":1.6758983863138937,"d":"1.68"},{"v":0.567228991,"d":"0.57"}]
["31151","Saline","NE",{"v":0.246003065,"d":"0.25"},{"v":1.56965700247716,"d":"1.57"},{"v":1.5696570024771597,"d":"1.57"},{"v":0.5200163939999999,"d":"0.52"}]
["31153","Sarpy","NE",{"v":0.16634659099999996,"d":"0.17"},{"v":1.421628289855001,"d":"1.42"},{"v":1.421628289855001,"d":"1.42"},{"v":0.42896350749999995,"d":"0.43"}]
["31155","Saunders","NE",{"v":0.25162136199999996,"d":"0.25"},{"v":1.6344749113306114,"d":"1.63"},{"v":1.6344749113306114,"d":"1.63"},{"v":0.531475152,"d":"0.53"}]
["31157","Scotts Bluff","NE",{"v":0.22834801699999996,"d":"0.23"},{"v":1.5987949130108703,"d":"1.60"},{"v":1.59879491301087,"d":"1.60"},{"v":0.48962977849999995,"d":"0.49"}]
["31159","Seward","NE",{"v":0.24638583299999997,"d":"0.25"},{"v":1.5997923483606447,"d":"1.60"},{"v":1.5997923483606444,"d":"1.60"},{"v":0.530555558,"d":"0.53"}]
["31161","Sheridan","NE",{"v":0.27692974,"d":"0.28"},{"v":1.6489642370500246,"d":"1.65"},{"v":1.6489642370500244,"d":"1.65"},{"v":0.5606847265,"d":"0.56"}]
["31163","Sherman","NE",{"v":0.275372986,"d":"0.28"},{"v":1.6603316808213824,"d":"1.66"},{"v":1.6603316808213824,"d":"1.66"},{"v":0.5632230939999999,"d":"0.56"}]
["31165","Sioux","NE",{"v":0.276041153,"d":"0.28"},{"v":1.6977952913466896,"d":"1.70"},{"v":1.6977952913466894,"d":"1.70"},{"v":0.56311514,"d":"0.56"}]
["31167","Stanton","NE",{"v":0.25514874199999993,"d":"0.26"},{"v":1.6812411554825186,"d":"1.68"},{"v":1.6812411554825184,"d":"1.68"},{"v":0.5561837764999998,"d":"0.56"}]
["31169","Thayer","NE",{"v":0.278478873,"d":"0.28"},{"v":1.5838458464841194,"d":"1.58"},{"v":1.5838458464841194,"d":"1.58"},{"v":0.5518329355,"d":"0.55"}]
["31171","Thomas","NE",{"v":0.272224551,"d":"0.27"},{"v":1.7098725075990462,"d":"1.71"},{"v":1.7098725075990462,"d":"1.71"},{"v":0.5632066905,"d":"0.56"}]
["31173","Thurston","NE",{"v":0.266429536,"d":"0.27"},{"v":1.6683976805491183,"d":"1.67"},{"v":1.6683976805491183,"d":"1.67"},{"v":0.581927746,"d":"0.58"}]
["31175","Valley","NE",{"v":0.273432514,"d":"0.27"},{"v":1.651231828732558,"d":"1.65"},{"v":1.6512318287325582,"d":"1.65"},{"v":0.5614717095,"d":"0.56"}]
["31177","Washington","NE",{"v":0.24102563,"d":"0.24"},{"v":1.6265058668659236,"d":"1.63"},{"v":1.6265058668659238,"d":"1.63"},{"v":0.5306736315,"d":"0.53"}]
["31179","Wayne","NE",{"v":0.23487611899999997,"d":"0.23"},{"v":1.6602698093200532,"d":"1.66"},{"v":1.6602698093200534,"d":"1.66"},{"v":0.51767067,"d":"0.52"}]
["31181","Webster","NE",{"v":0.281275194,"d":"0.28"},{"v":1.5620109310513564,"d":"1.56"},{"v":1.5620109310513561,"d":"1.56"},{"v":0.5545006055,"d":"0.55"}]
["31183","Wheeler","NE",{"v":0.274266293,"d":"0.27"},{"v":1.7278073147216024,"d":"1.73"},{"v":1.7278073147216024,"d":"1.73"},{"v":0.5691599770000001,"d":"0.57"}]
["31185","York","NE",{"v":0.234589321,"d":"0.23"},{"v":1.6053781334870574,"d":"1.61"},{"v":1.6053781334870574,"d":"1.61"},{"v":0.5045003445,"d":"0.50"}]
["32001","Churchill","NV",{"v":0.251259246,"d":"0.25"},{"v":1.596421019251291,"d":"1.60"},{"v":1.5964210192512913,"d":"1.60"},{"v":0.5059777835,"d":"0.51"}]
["32003","Clark","NV",{"v":0.22483936,"d":"0.22"},{"v":1.3074485264485527,"d":"1.31"},{"v":1.3074485264485527,"d":"1.31"},{"v":0.3972882375,"d":"0.40"}]
["32005","Douglas","NV",{"v":0.245700306,"d":"0.25"},{"v":1.5503567918676777,"d":"1.55"},{"v":1.5503567918676777,"d":"1.55"},{"v":0.5191325155000001,"d":"0.52"}]
["32007","Elko","NV",{"v":0.24345072400000003,"d":"0.24"},{"v":1.7247107491142881,"d":"1.72"},{"v":1.7247107491142883,"d":"1.72"},{"v":0.538151558,"d":"0.54"}]
["32009","Esmeralda","NV",{"v":0.281872993,"d":"0.28"},{"v":1.708301367244685,"d":"1.71"},{"v":1.7083013672446847,"d":"1.71"},{"v":0.571899247,"d":"0.57"}]
["32011","Eureka","NV",{"v":0.28943564999999993,"d":"0.29"},{"v":1.8032831851782072,"d":"1.80"},{"v":1.8032831851782074,"d":"1.80"},{"v":0.6134588935000002,"d":"0.61"}]
["32013","Humboldt","NV",{"v":0.24765769399999998,"d":"0.25"},{"v":1.652895278340705,"d":"1.65"},{"v":1.6528952783407047,"d":"1.65"},{"v":0.5151648934999999,"d":"0.52"}]
["32015","Lander","NV",{"v":0.24026112000000002,"d":"0.24"},{"v":1.7697992307235697,"d":"1.77"},{"v":1.7697992307235697,"d":"1.77"},{"v":0.5488005445,"d":"0.55"}]
["32017","Lincoln","NV",{"v":0.303764901,"d":"0.30"},{"v":1.6728688250660866,"d":"1.67"},{"v":1.6728688250660868,"d":"1.67"},{"v":0.5727208015,"d":"0.57"}]
["32019","Lyon","NV",{"v":0.24936324700000004,"d":"0.25"},{"v":1.5893871482540705,"d":"1.59"},{"v":1.5893871482540705,"d":"1.59"},{"v":0.518408172,"d":"0.52"}]
["32021","Mineral","NV",{"v":0.252857462,"d":"0.25"},{"v":1.6202801673393592,"d":"1.62"},{"v":1.6202801673393592,"d":"1.62"},{"v":0.500081796,"d":"0.50"}]
["32023","Nye","NV",{"v":0.24936763300000003,"d":"0.25"},{"v":1.6650952783672277,"d":"1.67"},{"v":1.665095278367228,"d":"1.67"},{"v":0.512509726,"d":"0.51"}]
["32027","Pershing","NV",{"v":0.285808856,"d":"0.29"},{"v":1.6970538446125114,"d":"1.70"},{"v":1.6970538446125112,"d":"1.70"},{"v":0.5787469614999999,"d":"0.58"}]
["32029","Storey","NV",{"v":0.292899077,"d":"0.29"},{"v":1.6809994145496103,"d":"1.68"},{"v":1.6809994145496105,"d":"1.68"},{"v":0.5676810364999999,"d":"0.57"}]
["32031","Washoe","NV",{"v":0.22154515300000002,"d":"0.22"},{"v":1.5631594420068706,"d":"1.56"},{"v":1.5631594420068704,"d":"1.56"},{"v":0.4536234325,"d":"0.45"}]
["32033","White Pine","NV",{"v":0.246865647,"d":"0.25"},{"v":1.7802481955923204,"d":"1.78"},{"v":1.7802481955923208,"d":"1.78"},{"v":0.5667169885,"d":"0.57"}]
["32510","Carson City","NV",{"v":0.195369172,"d":"0.20"},{"v":1.4886128527091573,"d":"1.49"},{"v":1.4886128527091573,"d":"1.49"},{"v":0.462598153,"d":"0.46"}]
["33001","Belknap","NH",{"v":0.420407863,"d":"0.42"},{"v":3.5832171368161756,"d":"3.58"},{"v":3.583217136816176,"d":"3.58"},{"v":1.4395085090000002,"d":"1.44"}]
["33003","Carroll","NH",{"v":0.44359938899999996,"d":"0.44"},{"v":3.6962861183449283,"d":"3.70"},{"v":3.6962861183449283,"d":"3.70"},{"v":1.6162645035,"d":"1.62"}]
["33005","Cheshire","NH",{"v":0.405152101,"d":"0.41"},{"v":3.6518955290322275,"d":"3.65"},{"v":3.651895529032227,"d":"3.65"},{"v":1.6034684305000002,"d":"1.60"}]
["33007","Coos","NH",{"v":0.40534510700000004,"d":"0.41"},{"v":3.9152390106651573,"d":"3.92"},{"v":3.9152390106651573,"d":"3.92"},{"v":1.6973814645,"d":"1.70"}]
["33009","Grafton","NH",{"v":0.411736996,"d":"0.41"},{"v":4.039101596122026,"d":"4.04"},{"v":4.039101596122025,"d":"4.04"},{"v":1.7025607339999997,"d":"1.70"}]
["33011","Hillsborough","NH",{"v":0.327005489,"d":"0.33"},{"v":3.269802764318011,"d":"3.27"},{"v":3.2698027643180105,"d":"3.27"},{"v":1.3402684589999998,"d":"1.34"}]
["33013","Merrimack","NH",{"v":0.3927825569999999,"d":"0.39"},{"v":3.519116392576862,"d":"3.52"},{"v":3.519116392576862,"d":"3.52"},{"v":1.493961733,"d":"1.49"}]
["33015","Rockingham","NH",{"v":0.3479376699999999,"d":"0.35"},{"v":3.4387008830056467,"d":"3.44"},{"v":3.438700883005646,"d":"3.44"},{"v":1.26338346,"d":"1.26"}]
["33017","Strafford","NH",{"v":0.359089928,"d":"0.36"},{"v":3.434762493767051,"d":"3.43"},{"v":3.4347624937670513,"d":"3.43"},{"v":1.3473726985,"d":"1.35"}]
["33019","Sullivan","NH",{"v":0.408564156,"d":"0.41"},{"v":3.6319682928306003,"d":"3.63"},{"v":3.6319682928306,"d":"3.63"},{"v":1.5862942765,"d":"1.59"}]
["34001","Atlantic","NJ",{"v":0.31997497300000005,"d":"0.32"},{"v":2.3969358648557897,"d":"2.40"},{"v":2.3969358648557897,"d":"2.40"},{"v":0.935678063,"d":"0.94"}]
["34003","Bergen","NJ",{"v":0.094818869,"d":"0.09"},{"v":1.749335308962509E-4,"d":"0.00"},{"v":1.7493353089625093E-4,"d":"0.00"},{"v":0.7229652440000001,"d":"0.72"}]
["34005","Burlington","NJ",{"v":0.3186513409999999,"d":"0.32"},{"v":2.4922876108436056,"d":"2.49"},{"v":2.492287610843605,"d":"2.49"},{"v":0.9833132730000002,"d":"0.98"}]
["34007","Camden","NJ",{"v":0.184751165,"d":"0.18"},{"v":0.07703564260342077,"d":"0.08"},{"v":0.07703564260342077,"d":"0.08"},{"v":0.784802537,"d":"0.78"}]
["34009","Cape May","NJ",{"v":0.40076708400000005,"d":"0.40"},{"v":2.5204502009769163,"d":"2.52"},{"v":2.5204502009769163,"d":"2.52"},{"v":0.8368385539999998,"d":"0.84"}]
["34011","Cumberland","NJ",{"v":0.35867910099999994,"d":"0.36"},{"v":2.479639060264931,"d":"2.48"},{"v":2.4796390602649305,"d":"2.48"},{"v":0.9292957605000001,"d":"0.93"}]
["34013","Essex","NJ",{"v":0.04733154400000001,"d":"0.05"},{"v":7.2868321305871036E-8,"d":"0.00"},{"v":7.2868321305871036E-8,"d":"0.00"},{"v":0.5903748924999999,"d":"0.59"}]
["34015","Gloucester","NJ",{"v":0.28833198900000007,"d":"0.29"},{"v":2.143811574854703,"d":"2.14"},{"v":2.143811574854703,"d":"2.14"},{"v":0.8636334329999998,"d":"0.86"}]
["34017","Hudson","NJ",{"v":2.8856980000000003E-3,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.31582435099999995,"d":"0.32"}]
["34019","Hunterdon","NJ",{"v":0.381976282,"d":"0.38"},{"v":2.7652778377007134,"d":"2.77"},{"v":2.7652778377007134,"d":"2.77"},{"v":1.063953928,"d":"1.06"}]
["34021","Mercer","NJ",{"v":0.23700147200000002,"d":"0.24"},{"v":0.8097349888132098,"d":"0.81"},{"v":0.8097349888132098,"d":"0.81"},{"v":0.7986993735,"d":"0.80"}]
["34023","Middlesex","NJ",{"v":0.157392777,"d":"0.16"},{"v":0.03577441887991463,"d":"0.04"},{"v":0.03577441887991463,"d":"0.04"},{"v":0.7226736625,"d":"0.72"}]
["34025","Monmouth","NJ",{"v":0.247911212,"d":"0.25"},{"v":1.2572577378646896,"d":"1.26"},{"v":1.2572577378646899,"d":"1.26"},{"v":0.7757505399999999,"d":"0.78"}]
["34027","Morris","NJ",{"v":0.24491325900000002,"d":"0.24"},{"v":2.0013706968289156,"d":"2.00"},{"v":2.001370696828916,"d":"2.00"},{"v":1.015851287,"d":"1.02"}]
["34029","Ocean","NJ",{"v":0.291316717,"d":"0.29"},{"v":2.0253452424409026,"d":"2.03"},{"v":2.025345242440902,"d":"2.03"},{"v":0.8012026805,"d":"0.80"}]
["34031","Passaic","NJ",{"v":0.135454503,"d":"0.14"},{"v":0.04767331972152028,"d":"0.05"},{"v":0.04767331972152028,"d":"0.05"},{"v":0.93841536,"d":"0.94"}]
["34033","Salem","NJ",{"v":0.40170258200000003,"d":"0.40"},{"v":2.599422060726465,"d":"2.60"},{"v":2.599422060726465,"d":"2.60"},{"v":0.9529264820000001,"d":"0.95"}]
["34035","Somerset","NJ",{"v":0.268706665,"d":"0.27"},{"v":2.0005574271764153,"d":"2.00"},{"v":2.0005574271764157,"d":"2.00"},{"v":0.8996762209999999,"d":"0.90"}]
["34037","Sussex","NJ",{"v":0.349204996,"d":"0.35"},{"v":2.8985389302018976,"d":"2.90"},{"v":2.8985389302018976,"d":"2.90"},{"v":1.1861637735,"d":"1.19"}]
["34039","Union","NJ",{"v":0.063295913,"d":"0.06"},{"v":3.8997342073335415E-6,"d":"0.00"},{"v":3.8997342073335406E-6,"d":"0.00"},{"v":0.6090874835000001,"d":"0.61"}]
["34041","Warren","NJ",{"v":0.35645935199999995,"d":"0.36"},{"v":2.7604637698699133,"d":"2.76"},{"v":2.7604637698699133,"d":"2.76"},{"v":1.124266971,"d":"1.12"}]
["35001","Bernalillo","NM",{"v":0.6814175490000001,"d":"0.68"},{"v":4.519289072551435,"d":"4.52"},{"v":4.519289072551434,"d":"4.52"},{"v":1.4939126649999999,"d":"1.49"}]
["35003","Catron","NM",{"v":0.9866015439999999,"d":"0.99"},{"v":5.969124185674487,"d":"5.97"},{"v":5.969124185674488,"d":"5.97"},{"v":2.1561249205000004,"d":"2.16"}]
["35005","Chaves","NM",{"v":0.8905378390000002,"d":"0.89"},{"v":4.959921446401252,"d":"4.96"},{"v":4.959921446401252,"d":"4.96"},{"v":1.6089378484999999,"d":"1.61"}]
["35006","Cibola","NM",{"v":0.8957511350000001,"d":"0.90"},{"v":5.6377362070545365,"d":"5.64"},{"v":5.6377362070545365,"d":"5.64"},{"v":1.9382464275000004,"d":"1.94"}]
["35007","Colfax","NM",{"v":0.8658404510000001,"d":"0.87"},{"v":5.739129568766698,"d":"5.74"},{"v":5.739129568766698,"d":"5.74"},{"v":1.988264175,"d":"1.99"}]
["35009","Curry","NM",{"v":0.867035597,"d":"0.87"},{"v":5.176961807987586,"d":"5.18"},{"v":5.176961807987585,"d":"5.18"},{"v":1.5671481229999997,"d":"1.57"}]
["35011","De Baca","NM",{"v":1.1095568870000003,"d":"1.11"},{"v":5.01677436660109,"d":"5.02"},{"v":5.01677436660109,"d":"5.02"},{"v":1.8453427820000001,"d":"1.85"}]
["35013","Dona Ana","NM",{"v":0.862637613,"d":"0.86"},{"v":4.699993300692445,"d":"4.70"},{"v":4.699993300692446,"d":"4.70"},{"v":1.5792828359999997,"d":"1.58"}]
["35015","Eddy","NM",{"v":0.8648601890000001,"d":"0.86"},{"v":4.957052993027366,"d":"4.96"},{"v":4.957052993027366,"d":"4.96"},{"v":1.6196170454999999,"d":"1.62"}]
["35017","Grant","NM",{"v":0.914365918,"d":"0.91"},{"v":4.975309582543496,"d":"4.98"},{"v":4.975309582543497,"d":"4.98"},{"v":1.7778903045000003,"d":"1.78"}]
["35019","Guadalupe","NM",{"v":0.9525075120000001,"d":"0.95"},{"v":5.319655585534566,"d":"5.32"},{"v":5.319655585534565,"d":"5.32"},{"v":1.7318298490000001,"d":"1.73"}]
["35021","Harding","NM",{"v":1.0634080909999999,"d":"1.06"},{"v":5.554125538803296,"d":"5.55"},{"v":5.554125538803296,"d":"5.55"},{"v":1.9125567175,"d":"1.91"}]
["35023","Hidalgo","NM",{"v":1.103917045,"d":"1.10"},{"v":5.103435214581494,"d":"5.10"},{"v":5.103435214581493,"d":"5.10"},{"v":1.835667924,"d":"1.84"}]
["35025","Lea","NM",{"v":0.8704807569999999,"d":"0.87"},{"v":5.023120075169345,"d":"5.02"},{"v":5.023120075169345,"d":"5.02"},{"v":1.5864314215000002,"d":"1.59"}]
["35027","Lincoln","NM",{"v":0.917495745,"d":"0.92"},{"v":5.355563244332923,"d":"5.36"},{"v":5.355563244332922,"d":"5.36"},{"v":1.8581172795,"d":"1.86"}]
["35028","Los Alamos","NM",{"v":0.745246263,"d":"0.75"},{"v":5.379849841181942,"d":"5.38"},{"v":5.379849841181942,"d":"5.38"},{"v":1.855204346,"d":"1.86"}]
["35029","Luna","NM",{"v":0.917535897,"d":"0.92"},{"v":5.0240007570315495,"d":"5.02"},{"v":5.0240007570315495,"d":"5.02"},{"v":1.660768318,"d":"1.66"}]
["35031","Mckinley","NM",{"v":0.90993382,"d":"0.91"},{"v":5.728476590789752,"d":"5.73"},{"v":5.728476590789752,"d":"5.73"},{"v":1.9001404665000001,"d":"1.90"}]
["35033","Mora","NM",{"v":0.9749822759999999,"d":"0.97"},{"v":6.161818387465537,"d":"6.16"},{"v":6.161818387465536,"d":"6.16"},{"v":2.157604629,"d":"2.16"}]
["35035","Otero","NM",{"v":0.8573800960000001,"d":"0.86"},{"v":5.458994133701157,"d":"5.46"},{"v":5.458994133701157,"d":"5.46"},{"v":1.790792849,"d":"1.79"}]
["35037","Quay","NM",{"v":0.9061145419999999,"d":"0.91"},{"v":5.334357968621081,"d":"5.33"},{"v":5.334357968621081,"d":"5.33"},{"v":1.737206543,"d":"1.74"}]
["35039","Rio Arriba","NM",{"v":0.845129922,"d":"0.85"},{"v":5.84234848958938,"d":"5.84"},{"v":5.84234848958938,"d":"5.84"},{"v":2.0464426185,"d":"2.05"}]
["35041","Roosevelt","NM",{"v":0.9195885569999999,"d":"0.92"},{"v":5.258914699073686,"d":"5.26"},{"v":5.258914699073685,"d":"5.26"},{"v":1.6916071334999998,"d":"1.69"}]
["35043","Sandoval","NM",{"v":0.801864723,"d":"0.80"},{"v":5.535831323419428,"d":"5.54"},{"v":5.535831323419428,"d":"5.54"},{"v":1.7780245705000002,"d":"1.78"}]
["35045","San Juan","NM",{"v":0.854194639,"d":"0.85"},{"v":5.621801935211528,"d":"5.62"},{"v":5.621801935211527,"d":"5.62"},{"v":1.770528068,"d":"1.77"}]
["35047","San Miguel","NM",{"v":0.855571261,"d":"0.86"},{"v":5.96298023824665,"d":"5.96"},{"v":5.962980238246649,"d":"5.96"},{"v":1.9701747624999995,"d":"1.97"}]
["35049","Santa Fe","NM",{"v":0.80415408,"d":"0.80"},{"v":5.610967167304772,"d":"5.61"},{"v":5.610967167304771,"d":"5.61"},{"v":1.8278525905,"d":"1.83"}]
["35051","Sierra","NM",{"v":0.88300918,"d":"0.88"},{"v":5.022034419024403,"d":"5.02"},{"v":5.022034419024403,"d":"5.02"},{"v":1.6738907105000003,"d":"1.67"}]
["35053","Socorro","NM",{"v":0.910636551,"d":"0.91"},{"v":5.268472072778609,"d":"5.27"},{"v":5.268472072778609,"d":"5.27"},{"v":1.7732385805000002,"d":"1.77"}]
["35055","Taos","NM",{"v":0.8650206649999999,"d":"0.87"},{"v":5.849652910278959,"d":"5.85"},{"v":5.84965291027896,"d":"5.85"},{"v":2.1146110485,"d":"2.11"}]
["35057","Torrance","NM",{"v":1.018220811,"d":"1.02"},{"v":5.587447545103282,"d":"5.59"},{"v":5.587447545103282,"d":"5.59"},{"v":1.9870521815000004,"d":"1.99"}]
["35059","Union","NM",{"v":1.0636882550000002,"d":"1.06"},{"v":5.156705404014214,"d":"5.16"},{"v":5.156705404014214,"d":"5.16"},{"v":1.9095913605000001,"d":"1.91"}]
["35061","Valencia","NM",{"v":0.8492706270000001,"d":"0.85"},{"v":5.003150777922021,"d":"5.00"},{"v":5.003150777922021,"d":"5.00"},{"v":1.5939108534999997,"d":"1.59"}]
["36001","Albany","NY",{"v":0.13927629799999997,"d":"0.14"},{"v":1.1638995889628325,"d":"1.16"},{"v":1.1638995889628325,"d":"1.16"},{"v":0.537605352,"d":"0.54"}]
["36003","Allegany","NY",{"v":0.1994416,"d":"0.20"},{"v":1.4850282554565453,"d":"1.49"},{"v":1.4850282554565453,"d":"1.49"},{"v":0.6444652405,"d":"0.64"}]
["36005","Bronx","NY",{"v":1.6600000000000002E-6,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.12539412800000002,"d":"0.13"}]
["36007","Broome","NY",{"v":0.15715161299999997,"d":"0.16"},{"v":1.3735759583623766,"d":"1.37"},{"v":1.3735759583623768,"d":"1.37"},{"v":0.581679888,"d":"0.58"}]
["36009","Cattaraugus","NY",{"v":0.18752139500000004,"d":"0.19"},{"v":1.473973535037977,"d":"1.47"},{"v":1.473973535037977,"d":"1.47"},{"v":0.6387954025,"d":"0.64"}]
["36011","Cayuga","NY",{"v":0.1932722,"d":"0.19"},{"v":1.4250043116013562,"d":"1.43"},{"v":1.4250043116013562,"d":"1.43"},{"v":0.52830291,"d":"0.53"}]
["36013","Chautauqua","NY",{"v":0.184140535,"d":"0.18"},{"v":1.3502954383573038,"d":"1.35"},{"v":1.3502954383573038,"d":"1.35"},{"v":0.554127223,"d":"0.55"}]
["36015","Chemung","NY",{"v":0.16324821,"d":"0.16"},{"v":1.3592512333369442,"d":"1.36"},{"v":1.3592512333369442,"d":"1.36"},{"v":0.5697730045,"d":"0.57"}]
["36017","Chenango","NY",{"v":0.197580173,"d":"0.20"},{"v":1.5798093258213692,"d":"1.58"},{"v":1.5798093258213692,"d":"1.58"},{"v":0.6543775465,"d":"0.65"}]
["36019","Clinton","NY",{"v":0.182998881,"d":"0.18"},{"v":1.636061393122864,"d":"1.64"},{"v":1.636061393122864,"d":"1.64"},{"v":0.6449859674999999,"d":"0.64"}]
["36021","Columbia","NY",{"v":0.19630564500000003,"d":"0.20"},{"v":1.4866057900644853,"d":"1.49"},{"v":1.4866057900644853,"d":"1.49"},{"v":0.6231973919999999,"d":"0.62"}]
["36023","Cortland","NY",{"v":0.17933657500000003,"d":"0.18"},{"v":1.4226736459514249,"d":"1.42"},{"v":1.4226736459514249,"d":"1.42"},{"v":0.5970606769999999,"d":"0.60"}]
["36025","Delaware","NY",{"v":0.19220304900000001,"d":"0.19"},{"v":1.6095488390357644,"d":"1.61"},{"v":1.6095488390357642,"d":"1.61"},{"v":0.6978248045000001,"d":"0.70"}]
["36027","Dutchess","NY",{"v":0.160021129,"d":"0.16"},{"v":1.4217283287052271,"d":"1.42"},{"v":1.4217283287052274,"d":"1.42"},{"v":0.5611456119999999,"d":"0.56"}]
["36029","Erie","NY",{"v":0.13094370399999997,"d":"0.13"},{"v":0.9640136251441603,"d":"0.96"},{"v":0.9640136251441603,"d":"0.96"},{"v":0.45916850500000006,"d":"0.46"}]
["36031","Essex","NY",{"v":0.185345261,"d":"0.19"},{"v":1.694584749089964,"d":"1.69"},{"v":1.694584749089964,"d":"1.69"},{"v":0.7495701164999998,"d":"0.75"}]
["36033","Franklin","NY",{"v":0.185119056,"d":"0.19"},{"v":1.6545373601027817,"d":"1.65"},{"v":1.6545373601027817,"d":"1.65"},{"v":0.6709761945000001,"d":"0.67"}]
["36035","Fulton","NY",{"v":0.174080453,"d":"0.17"},{"v":1.4780958871179357,"d":"1.48"},{"v":1.4780958871179357,"d":"1.48"},{"v":0.6587083595,"d":"0.66"}]
["36037","Genesee","NY",{"v":0.19605493200000002,"d":"0.20"},{"v":1.3939834898443144,"d":"1.39"},{"v":1.3939834898443144,"d":"1.39"},{"v":0.5418030505000001,"d":"0.54"}]
["36039","Greene","NY",{"v":0.18822515200000003,"d":"0.19"},{"v":1.6087447000517936,"d":"1.61"},{"v":1.6087447000517936,"d":"1.61"},{"v":0.7148391515,"d":"0.71"}]
["36041","Hamilton","NY",{"v":0.194753857,"d":"0.19"},{"v":1.7787179585614066,"d":"1.78"},{"v":1.7787179585614068,"d":"1.78"},{"v":0.772442835,"d":"0.77"}]
["36043","Herkimer","NY",{"v":0.17265096200000002,"d":"0.17"},{"v":1.6009695763064988,"d":"1.60"},{"v":1.6009695763064988,"d":"1.60"},{"v":0.6641203925,"d":"0.66"}]
["36045","Jefferson","NY",{"v":0.20076844300000002,"d":"0.20"},{"v":1.4585371010588737,"d":"1.46"},{"v":1.4585371010588737,"d":"1.46"},{"v":0.5090990365000001,"d":"0.51"}]
["36047","Kings","NY",{"v":1.06E-6,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.11346882949999999,"d":"0.11"}]
["36049","Lewis","NY",{"v":0.194449936,"d":"0.19"},{"v":1.7051916416117567,"d":"1.71"},{"v":1.7051916416117567,"d":"1.71"},{"v":0.688248142,"d":"0.69"}]
["36051","Livingston","NY",{"v":0.19344764100000003,"d":"0.19"},{"v":1.4460552016849193,"d":"1.45"},{"v":1.4460552016849193,"d":"1.45"},{"v":0.544425296,"d":"0.54"}]
["36053","Madison","NY",{"v":0.18965179499999998,"d":"0.19"},{"v":1.481842374092135,"d":"1.48"},{"v":1.481842374092135,"d":"1.48"},{"v":0.5705082765,"d":"0.57"}]
["36055","Monroe","NY",{"v":0.125042787,"d":"0.13"},{"v":0.8131816242306021,"d":"0.81"},{"v":0.8131816242306021,"d":"0.81"},{"v":0.412086376,"d":"0.41"}]
["36057","Montgomery","NY",{"v":0.18125033400000004,"d":"0.18"},{"v":1.365895896709025,"d":"1.37"},{"v":1.365895896709025,"d":"1.37"},{"v":0.5671713700000001,"d":"0.57"}]
["36059","Nassau","NY",{"v":0.04085044299999999,"d":"0.04"},{"v":2.9732448756199985E-5,"d":"0.00"},{"v":2.9732448756199988E-5,"d":"0.00"},{"v":0.264519759,"d":"0.26"}]
["36061","New York","NY",{"v":2.6699999999999997E-12,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.10887813049999999,"d":"0.11"}]
["36063","Niagara","NY",{"v":0.166339252,"d":"0.17"},{"v":1.2895898239815005,"d":"1.29"},{"v":1.2895898239815002,"d":"1.29"},{"v":0.452998058,"d":"0.45"}]
["36065","Oneida","NY",{"v":0.16790044600000004,"d":"0.17"},{"v":1.3868965167824083,"d":"1.39"},{"v":1.3868965167824086,"d":"1.39"},{"v":0.5686471240000001,"d":"0.57"}]
["36067","Onondaga","NY",{"v":0.14474892600000003,"d":"0.14"},{"v":1.2680806695200468,"d":"1.27"},{"v":1.268080669520047,"d":"1.27"},{"v":0.46978461949999994,"d":"0.47"}]
["36069","Ontario","NY",{"v":0.18897900000000004,"d":"0.19"},{"v":1.4276659608071363,"d":"1.43"},{"v":1.427665960807136,"d":"1.43"},{"v":0.5146103779999999,"d":"0.51"}]
["36071","Orange","NY",{"v":0.153984248,"d":"0.15"},{"v":1.3675324717199882,"d":"1.37"},{"v":1.3675324717199882,"d":"1.37"},{"v":0.555045723,"d":"0.56"}]
["36073","Orleans","NY",{"v":0.20242670700000007,"d":"0.20"},{"v":1.4371766272461304,"d":"1.44"},{"v":1.4371766272461306,"d":"1.44"},{"v":0.520430624,"d":"0.52"}]
["36075","Oswego","NY",{"v":0.189481187,"d":"0.19"},{"v":1.4617667954284588,"d":"1.46"},{"v":1.4617667954284586,"d":"1.46"},{"v":0.5787075754999998,"d":"0.58"}]
["36077","Otsego","NY",{"v":0.195594521,"d":"0.20"},{"v":1.5500318036142895,"d":"1.55"},{"v":1.5500318036142895,"d":"1.55"},{"v":0.6323697685,"d":"0.63"}]
["36079","Putnam","NY",{"v":0.15499448899999999,"d":"0.15"},{"v":1.471011778338159,"d":"1.47"},{"v":1.471011778338159,"d":"1.47"},{"v":0.5727489035000001,"d":"0.57"}]
["36081","Queens","NY",{"v":0.000176523,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.12620910900000007,"d":"0.13"}]
["36083","Rensselaer","NY",{"v":0.163669728,"d":"0.16"},{"v":1.3146326500406924,"d":"1.31"},{"v":1.3146326500406926,"d":"1.31"},{"v":0.5817305125000002,"d":"0.58"}]
["36085","Richmond","NY",{"v":0.016059833,"d":"0.02"},{"v":6.220629165802031e-11,"d":"0.00"},{"v":6.220629165802031e-11,"d":"0.00"},{"v":0.209893479,"d":"0.21"}]
["36087","Rockland","NY",{"v":0.093934625,"d":"0.09"},{"v":0.4176506631771431,"d":"0.42"},{"v":0.41765066317714317,"d":"0.42"},{"v":0.450221095,"d":"0.45"}]
["36089","St Lawrence","NY",{"v":0.18969643700000002,"d":"0.19"},{"v":1.5893668349962093,"d":"1.59"},{"v":1.5893668349962093,"d":"1.59"},{"v":0.6281010890000001,"d":"0.63"}]
["36091","Saratoga","NY",{"v":0.161746622,"d":"0.16"},{"v":1.3852236081024278,"d":"1.39"},{"v":1.3852236081024278,"d":"1.39"},{"v":0.595556549,"d":"0.60"}]
["36093","Schenectady","NY",{"v":0.13006545,"d":"0.13"},{"v":1.1263974267797714,"d":"1.13"},{"v":1.1263974267797714,"d":"1.13"},{"v":0.5158606555,"d":"0.52"}]
["36095","Schoharie","NY",{"v":0.196745645,"d":"0.20"},{"v":1.598421333375481,"d":"1.60"},{"v":1.5984213333754813,"d":"1.60"},{"v":0.6729308255,"d":"0.67"}]
["36097","Schuyler","NY",{"v":0.20176769800000002,"d":"0.20"},{"v":1.5430777190613132,"d":"1.54"},{"v":1.543077719061313,"d":"1.54"},{"v":0.605687218,"d":"0.61"}]
["36099","Seneca","NY",{"v":0.20044317599999997,"d":"0.20"},{"v":1.446949035756615,"d":"1.45"},{"v":1.446949035756615,"d":"1.45"},{"v":0.503359586,"d":"0.50"}]
["36101","Steuben","NY",{"v":0.188564319,"d":"0.19"},{"v":1.460579952624293,"d":"1.46"},{"v":1.460579952624293,"d":"1.46"},{"v":0.5971784809999999,"d":"0.60"}]
["36103","Suffolk","NY",{"v":0.11483847799999998,"d":"0.11"},{"v":0.5275395912126353,"d":"0.53"},{"v":0.5275395912126353,"d":"0.53"},{"v":0.344821063,"d":"0.34"}]
["36105","Sullivan","NY",{"v":0.184767025,"d":"0.18"},{"v":1.6122402047461657,"d":"1.61"},{"v":1.6122402047461657,"d":"1.61"},{"v":0.7191421399999999,"d":"0.72"}]
["36107","Tioga","NY",{"v":0.187263302,"d":"0.19"},{"v":1.525936534102294,"d":"1.53"},{"v":1.5259365341022941,"d":"1.53"},{"v":0.6190875925,"d":"0.62"}]
["36109","Tompkins","NY",{"v":0.17381196,"d":"0.17"},{"v":1.407156873202833,"d":"1.41"},{"v":1.407156873202833,"d":"1.41"},{"v":0.5583316195,"d":"0.56"}]
["36111","Ulster","NY",{"v":0.16620724299999998,"d":"0.17"},{"v":1.5535139823342974,"d":"1.55"},{"v":1.5535139823342972,"d":"1.55"},{"v":0.6938488890000002,"d":"0.69"}]
["36113","Warren","NY",{"v":0.161539458,"d":"0.16"},{"v":1.5671891302721621,"d":"1.57"},{"v":1.5671891302721623,"d":"1.57"},{"v":0.708064126,"d":"0.71"}]
["36115","Washington","NY",{"v":0.196730995,"d":"0.20"},{"v":1.4604568501526818,"d":"1.46"},{"v":1.4604568501526818,"d":"1.46"},{"v":0.603216979,"d":"0.60"}]
["36117","Wayne","NY",{"v":0.19432888199999998,"d":"0.19"},{"v":1.4307327062719037,"d":"1.43"},{"v":1.4307327062719035,"d":"1.43"},{"v":0.544995453,"d":"0.54"}]
["36119","Westchester","NY",{"v":0.077509242,"d":"0.08"},{"v":0.0608007767547405,"d":"0.06"},{"v":0.0608007767547405,"d":"0.06"},{"v":0.43776908550000004,"d":"0.44"}]
["36121","Wyoming","NY",{"v":0.202085512,"d":"0.20"},{"v":1.4450429934787672,"d":"1.45"},{"v":1.4450429934787672,"d":"1.45"},{"v":0.5697080570000002,"d":"0.57"}]
["36123","Yates","NY",{"v":0.20573481,"d":"0.21"},{"v":1.4891336655631704,"d":"1.49"},{"v":1.4891336655631706,"d":"1.49"},{"v":0.5424190710000002,"d":"0.54"}]
["37001","Alamance","NC",{"v":0.205036201,"d":"0.21"},{"v":1.477014974765208,"d":"1.48"},{"v":1.4770149747652077,"d":"1.48"},{"v":0.6154647965,"d":"0.62"}]
["37003","Alexander","NC",{"v":0.24588423000000006,"d":"0.25"},{"v":1.613074533802636,"d":"1.61"},{"v":1.6130745338026358,"d":"1.61"},{"v":0.6949204495000001,"d":"0.69"}]
["37005","Alleghany","NC",{"v":0.262165891,"d":"0.26"},{"v":1.7040789521004591,"d":"1.70"},{"v":1.7040789521004591,"d":"1.70"},{"v":0.7791942230000001,"d":"0.78"}]
["37007","Anson","NC",{"v":0.25412901499999996,"d":"0.25"},{"v":1.592387496236094,"d":"1.59"},{"v":1.5923874962360938,"d":"1.59"},{"v":0.7237546585,"d":"0.72"}]
["37009","Ashe","NC",{"v":0.24310438799999998,"d":"0.24"},{"v":1.7121289399174027,"d":"1.71"},{"v":1.7121289399174027,"d":"1.71"},{"v":0.806379058,"d":"0.81"}]
["37011","Avery","NC",{"v":0.24580003500000003,"d":"0.25"},{"v":1.7250910801760482,"d":"1.73"},{"v":1.725091080176048,"d":"1.73"},{"v":0.866356025,"d":"0.87"}]
["37013","Beaufort","NC",{"v":0.261141386,"d":"0.26"},{"v":1.5331440556850555,"d":"1.53"},{"v":1.5331440556850557,"d":"1.53"},{"v":0.6203304079999999,"d":"0.62"}]
["37015","Bertie","NC",{"v":0.263901844,"d":"0.26"},{"v":1.6205971128916123,"d":"1.62"},{"v":1.6205971128916123,"d":"1.62"},{"v":0.7103007200000002,"d":"0.71"}]
["37017","Bladen","NC",{"v":0.266692038,"d":"0.27"},{"v":1.5604992879394728,"d":"1.56"},{"v":1.5604992879394726,"d":"1.56"},{"v":0.7173453765,"d":"0.72"}]
["37019","Brunswick","NC",{"v":0.23764398600000003,"d":"0.24"},{"v":1.5442387472754249,"d":"1.54"},{"v":1.5442387472754249,"d":"1.54"},{"v":0.6022924955000001,"d":"0.60"}]
["37021","Buncombe","NC",{"v":0.187862055,"d":"0.19"},{"v":1.598379885957544,"d":"1.60"},{"v":1.5983798859575442,"d":"1.60"},{"v":0.6974812105,"d":"0.70"}]
["37023","Burke","NC",{"v":0.21224097300000003,"d":"0.21"},{"v":1.6771572528467227,"d":"1.68"},{"v":1.6771572528467227,"d":"1.68"},{"v":0.730906235,"d":"0.73"}]
["37025","Cabarrus","NC",{"v":0.19413487800000004,"d":"0.19"},{"v":1.38911815973629,"d":"1.39"},{"v":1.38911815973629,"d":"1.39"},{"v":0.5842420475000001,"d":"0.58"}]
["37027","Caldwell","NC",{"v":0.206470688,"d":"0.21"},{"v":1.6678774888340067,"d":"1.67"},{"v":1.6678774888340067,"d":"1.67"},{"v":0.746164154,"d":"0.75"}]
["37029","Camden","NC",{"v":0.28884831899999996,"d":"0.29"},{"v":1.5790485768683813,"d":"1.58"},{"v":1.5790485768683813,"d":"1.58"},{"v":0.6431815625,"d":"0.64"}]
["37031","Carteret","NC",{"v":0.247436951,"d":"0.25"},{"v":1.509604807149919,"d":"1.51"},{"v":1.5096048071499193,"d":"1.51"},{"v":0.49982606450000006,"d":"0.50"}]
["37033","Caswell","NC",{"v":0.264578556,"d":"0.26"},{"v":1.6608910195414641,"d":"1.66"},{"v":1.6608910195414641,"d":"1.66"},{"v":0.75271408,"d":"0.75"}]
["37035","Catawba","NC",{"v":0.208313425,"d":"0.21"},{"v":1.5070044502575142,"d":"1.51"},{"v":1.5070044502575142,"d":"1.51"},{"v":0.587055121,"d":"0.59"}]
["37037","Chatham","NC",{"v":0.243229517,"d":"0.24"},{"v":1.557762340482866,"d":"1.56"},{"v":1.5577623404828658,"d":"1.56"},{"v":0.7270740480000001,"d":"0.73"}]
["37039","Cherokee","NC",{"v":0.250091528,"d":"0.25"},{"v":1.7231722042582045,"d":"1.72"},{"v":1.723172204258204,"d":"1.72"},{"v":0.8644591010000001,"d":"0.86"}]
["37041","Chowan","NC",{"v":0.270953721,"d":"0.27"},{"v":1.560901415718984,"d":"1.56"},{"v":1.560901415718984,"d":"1.56"},{"v":0.5864579145,"d":"0.59"}]
["37043","Clay","NC",{"v":0.252762923,"d":"0.25"},{"v":1.724521377355198,"d":"1.72"},{"v":1.724521377355198,"d":"1.72"},{"v":0.8520611750000002,"d":"0.85"}]
["37045","Cleveland","NC",{"v":0.23599084800000003,"d":"0.24"},{"v":1.5088669038863687,"d":"1.51"},{"v":1.508866903886369,"d":"1.51"},{"v":0.6423876410000001,"d":"0.64"}]
["37047","Columbus","NC",{"v":0.262648106,"d":"0.26"},{"v":1.567372190573355,"d":"1.57"},{"v":1.567372190573355,"d":"1.57"},{"v":0.6944089415,"d":"0.69"}]
["37049","Craven","NC",{"v":0.227098891,"d":"0.23"},{"v":1.5245880303019783,"d":"1.52"},{"v":1.5245880303019779,"d":"1.52"},{"v":0.6266060975000002,"d":"0.63"}]
["37051","Cumberland","NC",{"v":0.191997793,"d":"0.19"},{"v":1.4156841471089487,"d":"1.42"},{"v":1.415684147108949,"d":"1.42"},{"v":0.5607038995,"d":"0.56"}]
["37053","Currituck","NC",{"v":0.300296073,"d":"0.30"},{"v":1.5493706983487021,"d":"1.55"},{"v":1.5493706983487021,"d":"1.55"},{"v":0.5694295075000001,"d":"0.57"}]
["37055","Dare","NC",{"v":0.24994635,"d":"0.25"},{"v":1.517578024479777,"d":"1.52"},{"v":1.517578024479777,"d":"1.52"},{"v":0.5010343155,"d":"0.50"}]
["37057","Davidson","NC",{"v":0.22233262899999998,"d":"0.22"},{"v":1.5359220528906807,"d":"1.54"},{"v":1.5359220528906807,"d":"1.54"},{"v":0.6509227184999999,"d":"0.65"}]
["37059","Davie","NC",{"v":0.24843719799999997,"d":"0.25"},{"v":1.5893682506606255,"d":"1.59"},{"v":1.5893682506606255,"d":"1.59"},{"v":0.6653794025000002,"d":"0.67"}]
["37061","Duplin","NC",{"v":0.268403726,"d":"0.27"},{"v":1.569746273886622,"d":"1.57"},{"v":1.5697462738866217,"d":"1.57"},{"v":0.6667311229999999,"d":"0.67"}]
["37063","Durham","NC",{"v":0.149017785,"d":"0.15"},{"v":1.0395491126384009,"d":"1.04"},{"v":1.0395491126384009,"d":"1.04"},{"v":0.5984084225,"d":"0.60"}]
["37065","Edgecombe","NC",{"v":0.238722045,"d":"0.24"},{"v":1.492651491894031,"d":"1.49"},{"v":1.4926514918940312,"d":"1.49"},{"v":0.61825595,"d":"0.62"}]
["37067","Forsyth","NC",{"v":0.16180897,"d":"0.16"},{"v":1.24875551209824,"d":"1.25"},{"v":1.2487555120982403,"d":"1.25"},{"v":0.5526852435,"d":"0.55"}]
["37069","Franklin","NC",{"v":0.250768711,"d":"0.25"},{"v":1.6303849599576676,"d":"1.63"},{"v":1.6303849599576676,"d":"1.63"},{"v":0.7296718289999999,"d":"0.73"}]
["37071","Gaston","NC",{"v":0.186933978,"d":"0.19"},{"v":1.3778741807250297,"d":"1.38"},{"v":1.3778741807250299,"d":"1.38"},{"v":0.5923086755000001,"d":"0.59"}]
["37073","Gates","NC",{"v":0.272016345,"d":"0.27"},{"v":1.6118475703707686,"d":"1.61"},{"v":1.6118475703707684,"d":"1.61"},{"v":0.7313694559999999,"d":"0.73"}]
["37075","Graham","NC",{"v":0.24642177499999998,"d":"0.25"},{"v":1.7487651064549226,"d":"1.75"},{"v":1.7487651064549223,"d":"1.75"},{"v":0.9055037805000001,"d":"0.91"}]
["37077","Granville","NC",{"v":0.23663671099999997,"d":"0.24"},{"v":1.6113877896653277,"d":"1.61"},{"v":1.611387789665328,"d":"1.61"},{"v":0.7248410770000001,"d":"0.72"}]
["37079","Greene","NC",{"v":0.28484595800000007,"d":"0.28"},{"v":1.5768300180561934,"d":"1.58"},{"v":1.5768300180561932,"d":"1.58"},{"v":0.6348569095000001,"d":"0.63"}]
["37081","Guilford","NC",{"v":0.169828136,"d":"0.17"},{"v":1.3090446677929797,"d":"1.31"},{"v":1.3090446677929801,"d":"1.31"},{"v":0.5553323265000002,"d":"0.56"}]
["37083","Halifax","NC",{"v":0.242204892,"d":"0.24"},{"v":1.536653734743571,"d":"1.54"},{"v":1.536653734743571,"d":"1.54"},{"v":0.6695945480000001,"d":"0.67"}]
["37085","Harnett","NC",{"v":0.24474607599999998,"d":"0.24"},{"v":1.5143135405330845,"d":"1.51"},{"v":1.5143135405330845,"d":"1.51"},{"v":0.6337142829999999,"d":"0.63"}]
["37087","Haywood","NC",{"v":0.22141647500000003,"d":"0.22"},{"v":1.6976201013173702,"d":"1.70"},{"v":1.6976201013173704,"d":"1.70"},{"v":0.8033520925,"d":"0.80"}]
["37089","Henderson","NC",{"v":0.203706735,"d":"0.20"},{"v":1.6120752964228862,"d":"1.61"},{"v":1.6120752964228862,"d":"1.61"},{"v":0.7127402055,"d":"0.71"}]
["37091","Hertford","NC",{"v":0.251355843,"d":"0.25"},{"v":1.537149490798686,"d":"1.54"},{"v":1.537149490798686,"d":"1.54"},{"v":0.6879378025,"d":"0.69"}]
["37093","Hoke","NC",{"v":0.23716879800000004,"d":"0.24"},{"v":1.5081559363714663,"d":"1.51"},{"v":1.5081559363714663,"d":"1.51"},{"v":0.6174920675000001,"d":"0.62"}]
["37095","Hyde","NC",{"v":0.301579875,"d":"0.30"},{"v":1.5259640587451193,"d":"1.53"},{"v":1.525964058745119,"d":"1.53"},{"v":0.5977711535,"d":"0.60"}]
["37097","Iredell","NC",{"v":0.220959133,"d":"0.22"},{"v":1.5158467448869708,"d":"1.52"},{"v":1.5158467448869706,"d":"1.52"},{"v":0.6041203169999999,"d":"0.60"}]
["37099","Jackson","NC",{"v":0.23136702800000003,"d":"0.23"},{"v":1.714865534127831,"d":"1.71"},{"v":1.7148655341278312,"d":"1.71"},{"v":0.8511442175,"d":"0.85"}]
["37101","Johnston","NC",{"v":0.23918607399999997,"d":"0.24"},{"v":1.5068525629890943,"d":"1.51"},{"v":1.5068525629890943,"d":"1.51"},{"v":0.6185699944999999,"d":"0.62"}]
["37103","Jones","NC",{"v":0.273787592,"d":"0.27"},{"v":1.5779932558580563,"d":"1.58"},{"v":1.5779932558580565,"d":"1.58"},{"v":0.7309900245000001,"d":"0.73"}]
["37105","Lee","NC",{"v":0.21560160999999997,"d":"0.22"},{"v":1.5505527578651959,"d":"1.55"},{"v":1.5505527578651956,"d":"1.55"},{"v":0.694236123,"d":"0.69"}]
["37107","Lenoir","NC",{"v":0.238559608,"d":"0.24"},{"v":1.4873947479006238,"d":"1.49"},{"v":1.4873947479006238,"d":"1.49"},{"v":0.5936132565,"d":"0.59"}]
["37109","Lincoln","NC",{"v":0.23270156199999997,"d":"0.23"},{"v":1.5181870934597714,"d":"1.52"},{"v":1.5181870934597712,"d":"1.52"},{"v":0.627958118,"d":"0.63"}]
["37111","McDowell","NC",{"v":0.226447955,"d":"0.23"},{"v":1.7322572190755665,"d":"1.73"},{"v":1.7322572190755665,"d":"1.73"},{"v":0.8161385265000001,"d":"0.82"}]
["37113","Macon","NC",{"v":0.236839557,"d":"0.24"},{"v":1.7069817538152119,"d":"1.71"},{"v":1.7069817538152119,"d":"1.71"},{"v":0.859048744,"d":"0.86"}]
["37115","Madison","NC",{"v":0.24994127500000002,"d":"0.25"},{"v":1.7251216753643785,"d":"1.73"},{"v":1.7251216753643788,"d":"1.73"},{"v":0.8363968515,"d":"0.84"}]
["37117","Martin","NC",{"v":0.261721577,"d":"0.26"},{"v":1.5738548414039917,"d":"1.57"},{"v":1.5738548414039917,"d":"1.57"},{"v":0.6834878094999999,"d":"0.68"}]
["37119","Mecklenburg","NC",{"v":0.11543168899999999,"d":"0.12"},{"v":0.10389743441817352,"d":"0.10"},{"v":0.10389743441817352,"d":"0.10"},{"v":0.48314997350000005,"d":"0.48"}]
["37121","Mitchell","NC",{"v":0.23956328499999996,"d":"0.24"},{"v":1.7119143769023306,"d":"1.71"},{"v":1.7119143769023304,"d":"1.71"},{"v":0.8507754899999999,"d":"0.85"}]
["37123","Montgomery","NC",{"v":0.24888400299999996,"d":"0.25"},{"v":1.5962736808304616,"d":"1.60"},{"v":1.5962736808304614,"d":"1.60"},{"v":0.770898653,"d":"0.77"}]
["37125","Moore","NC",{"v":0.23323276200000004,"d":"0.23"},{"v":1.5666508661711156,"d":"1.57"},{"v":1.5666508661711156,"d":"1.57"},{"v":0.6868915910000001,"d":"0.69"}]
["37127","Nash","NC",{"v":0.23535104799999998,"d":"0.24"},{"v":1.511147037309234,"d":"1.51"},{"v":1.5111470373092342,"d":"1.51"},{"v":0.6337004475,"d":"0.63"}]
["37129","New Hanover","NC",{"v":0.16507271200000004,"d":"0.17"},{"v":0.8137204283012327,"d":"0.81"},{"v":0.8137204283012326,"d":"0.81"},{"v":0.4382939679999999,"d":"0.44"}]
["37131","Northampton","NC",{"v":0.269808335,"d":"0.27"},{"v":1.5895365955615104,"d":"1.59"},{"v":1.5895365955615102,"d":"1.59"},{"v":0.7008060755000001,"d":"0.70"}]
["37133","Onslow","NC",{"v":0.230124402,"d":"0.23"},{"v":1.5264321359941346,"d":"1.53"},{"v":1.5264321359941344,"d":"1.53"},{"v":0.58415332,"d":"0.58"}]
["37135","Orange","NC",{"v":0.19840130900000003,"d":"0.20"},{"v":1.5300195874489542,"d":"1.53"},{"v":1.5300195874489542,"d":"1.53"},{"v":0.674400442,"d":"0.67"}]
["37137","Pamlico","NC",{"v":0.296676758,"d":"0.30"},{"v":1.5571246389253763,"d":"1.56"},{"v":1.5571246389253766,"d":"1.56"},{"v":0.624843376,"d":"0.62"}]
["37139","Pasquotank","NC",{"v":0.24414937600000003,"d":"0.24"},{"v":1.5190789498043673,"d":"1.52"},{"v":1.5190789498043673,"d":"1.52"},{"v":0.5494355965000001,"d":"0.55"}]
["37141","Pender","NC",{"v":0.25240566,"d":"0.25"},{"v":1.5734605265867798,"d":"1.57"},{"v":1.5734605265867794,"d":"1.57"},{"v":0.7064002395000001,"d":"0.71"}]
["37143","Perquimans","NC",{"v":0.296573749,"d":"0.30"},{"v":1.567688403693063,"d":"1.57"},{"v":1.5676884036930627,"d":"1.57"},{"v":0.60394658,"d":"0.60"}]
["37145","Person","NC",{"v":0.249532669,"d":"0.25"},{"v":1.6077437525623464,"d":"1.61"},{"v":1.6077437525623464,"d":"1.61"},{"v":0.7197307775,"d":"0.72"}]
["37147","Pitt","NC",{"v":0.212708222,"d":"0.21"},{"v":1.4827672582442983,"d":"1.48"},{"v":1.4827672582442986,"d":"1.48"},{"v":0.5597446604999999,"d":"0.56"}]
["37149","Polk","NC",{"v":0.24874105100000002,"d":"0.25"},{"v":1.6886179625023714,"d":"1.69"},{"v":1.6886179625023714,"d":"1.69"},{"v":0.7975139489999999,"d":"0.80"}]
["37151","Randolph","NC",{"v":0.23015485300000002,"d":"0.23"},{"v":1.564851348395962,"d":"1.56"},{"v":1.5648513483959618,"d":"1.56"},{"v":0.68864561,"d":"0.69"}]
["37153","Richmond","NC",{"v":0.23022514500000002,"d":"0.23"},{"v":1.5402691339372165,"d":"1.54"},{"v":1.5402691339372165,"d":"1.54"},{"v":0.6809622715,"d":"0.68"}]
["37155","Robeson","NC",{"v":0.247841989,"d":"0.25"},{"v":1.5366233883700977,"d":"1.54"},{"v":1.5366233883700977,"d":"1.54"},{"v":0.619606371,"d":"0.62"}]
["37157","Rockingham","NC",{"v":0.23390161399999998,"d":"0.23"},{"v":1.5660820202834842,"d":"1.57"},{"v":1.5660820202834842,"d":"1.57"},{"v":0.695176039,"d":"0.70"}]
["37159","Rowan","NC",{"v":0.21957348,"d":"0.22"},{"v":1.516406885402298,"d":"1.52"},{"v":1.516406885402298,"d":"1.52"},{"v":0.6225588175000002,"d":"0.62"}]
["37161","Rutherford","NC",{"v":0.231329656,"d":"0.23"},{"v":1.6830235297461689,"d":"1.68"},{"v":1.6830235297461689,"d":"1.68"},{"v":0.737925531,"d":"0.74"}]
["37163","Sampson","NC",{"v":0.270911657,"d":"0.27"},{"v":1.556523366040034,"d":"1.56"},{"v":1.5565233660400337,"d":"1.56"},{"v":0.6486939315000001,"d":"0.65"}]
["37165","Scotland","NC",{"v":0.240049492,"d":"0.24"},{"v":1.5006112765582602,"d":"1.50"},{"v":1.50061127655826,"d":"1.50"},{"v":0.6256702694999999,"d":"0.63"}]
["37167","Stanly","NC",{"v":0.250077119,"d":"0.25"},{"v":1.5393476425997927,"d":"1.54"},{"v":1.5393476425997927,"d":"1.54"},{"v":0.6533686125000001,"d":"0.65"}]
["37169","Stokes","NC",{"v":0.24435311000000004,"d":"0.24"},{"v":1.6504710045017836,"d":"1.65"},{"v":1.6504710045017832,"d":"1.65"},{"v":0.7367564249999999,"d":"0.74"}]
["37171","Surry","NC",{"v":0.23682211399999997,"d":"0.24"},{"v":1.7010364247187248,"d":"1.70"},{"v":1.7010364247187248,"d":"1.70"},{"v":0.7038985394999999,"d":"0.70"}]
["37173","Swain","NC",{"v":0.24680969999999997,"d":"0.25"},{"v":1.7458589900742183,"d":"1.75"},{"v":1.7458589900742183,"d":"1.75"},{"v":0.9013965199999999,"d":"0.90"}]
["37175","Transylvania","NC",{"v":0.22412866,"d":"0.22"},{"v":1.6699276222999728,"d":"1.67"},{"v":1.6699276222999728,"d":"1.67"},{"v":0.8412198289999999,"d":"0.84"}]
["37177","Tyrrell","NC",{"v":0.283728766,"d":"0.28"},{"v":1.5982279191721736,"d":"1.60"},{"v":1.598227919172173,"d":"1.60"},{"v":0.6764720445,"d":"0.68"}]
["37179","Union","NC",{"v":0.217570387,"d":"0.22"},{"v":1.4241262133291017,"d":"1.42"},{"v":1.4241262133291017,"d":"1.42"},{"v":0.5835886515,"d":"0.58"}]
["37181","Vance","NC",{"v":0.22745678100000002,"d":"0.23"},{"v":1.5825416356042343,"d":"1.58"},{"v":1.582541635604234,"d":"1.58"},{"v":0.6840043795000001,"d":"0.68"}]
["37183","Wake","NC",{"v":0.14989055199999998,"d":"0.15"},{"v":0.9150421940109076,"d":"0.92"},{"v":0.9150421940109076,"d":"0.92"},{"v":0.5447315420000001,"d":"0.54"}]
["37185","Warren","NC",{"v":0.261728623,"d":"0.26"},{"v":1.6689631905188067,"d":"1.67"},{"v":1.6689631905188071,"d":"1.67"},{"v":0.768865869,"d":"0.77"}]
["37187","Washington","NC",{"v":0.267531063,"d":"0.27"},{"v":1.5173862234704119,"d":"1.52"},{"v":1.5173862234704119,"d":"1.52"},{"v":0.6138839060000002,"d":"0.61"}]
["37189","Watauga","NC",{"v":0.21392385300000002,"d":"0.21"},{"v":1.6727587618875122,"d":"1.67"},{"v":1.6727587618875122,"d":"1.67"},{"v":0.796615781,"d":"0.80"}]
["37191","Wayne","NC",{"v":0.23725951200000006,"d":"0.24"},{"v":1.508699383277463,"d":"1.51"},{"v":1.5086993832774627,"d":"1.51"},{"v":0.575983821,"d":"0.58"}]
["37193","Wilkes","NC",{"v":0.235343341,"d":"0.24"},{"v":1.7224845539755946,"d":"1.72"},{"v":1.722484553975595,"d":"1.72"},{"v":0.7668757585,"d":"0.77"}]
["37195","Wilson","NC",{"v":0.234372229,"d":"0.23"},{"v":1.3826863822943514,"d":"1.38"},{"v":1.3826863822943514,"d":"1.38"},{"v":0.5826327085,"d":"0.58"}]
["37197","Yadkin","NC",{"v":0.254562091,"d":"0.25"},{"v":1.6955767734069735,"d":"1.70"},{"v":1.6955767734069738,"d":"1.70"},{"v":0.6956229499999999,"d":"0.70"}]
["37199","Yancey","NC",{"v":0.248539383,"d":"0.25"},{"v":1.7229958859217758,"d":"1.72"},{"v":1.722995885921776,"d":"1.72"},{"v":0.8725814570000002,"d":"0.87"}]
["38001","Adams","ND",{"v":0.061481537,"d":"0.06"},{"v":0.4283313141179481,"d":"0.43"},{"v":0.4283313141179482,"d":"0.43"},{"v":0.140025776,"d":"0.14"}]
["38003","Barnes","ND",{"v":0.051219447999999994,"d":"0.05"},{"v":0.42983316251538645,"d":"0.43"},{"v":0.4298331625153865,"d":"0.43"},{"v":0.126721179,"d":"0.13"}]
["38005","Benson","ND",{"v":0.059859691,"d":"0.06"},{"v":0.442811932521392,"d":"0.44"},{"v":0.442811932521392,"d":"0.44"},{"v":0.1461184145,"d":"0.15"}]
["38007","Billings","ND",{"v":0.061592601999999996,"d":"0.06"},{"v":0.43346267969933705,"d":"0.43"},{"v":0.43346267969933705,"d":"0.43"},{"v":0.141915637,"d":"0.14"}]
["38009","Bottineau","ND",{"v":0.060283083999999994,"d":"0.06"},{"v":0.445632183360073,"d":"0.45"},{"v":0.44563218336007293,"d":"0.45"},{"v":0.14535369100000003,"d":"0.15"}]
["38011","Bowman","ND",{"v":0.060552624000000006,"d":"0.06"},{"v":0.4210759491602747,"d":"0.42"},{"v":0.4210759491602747,"d":"0.42"},{"v":0.1405180905,"d":"0.14"}]
["38013","Burke","ND",{"v":0.06090736000000001,"d":"0.06"},{"v":0.443261178389634,"d":"0.44"},{"v":0.443261178389634,"d":"0.44"},{"v":0.144025838,"d":"0.14"}]
["38015","Burleigh","ND",{"v":0.047620527,"d":"0.05"},{"v":0.41191097371140784,"d":"0.41"},{"v":0.41191097371140795,"d":"0.41"},{"v":0.11609446500000002,"d":"0.12"}]
["38017","Cass","ND",{"v":0.04300548199999999,"d":"0.04"},{"v":0.41933270992979915,"d":"0.42"},{"v":0.4193327099297992,"d":"0.42"},{"v":0.11361815300000001,"d":"0.11"}]
["38019","Cavalier","ND",{"v":0.060124355000000004,"d":"0.06"},{"v":0.4446594155761879,"d":"0.44"},{"v":0.4446594155761878,"d":"0.44"},{"v":0.1454380865,"d":"0.15"}]
["38021","Dickey","ND",{"v":0.059698777,"d":"0.06"},{"v":0.43346158870658036,"d":"0.43"},{"v":0.4334615887065804,"d":"0.43"},{"v":0.140991147,"d":"0.14"}]
["38023","Divide","ND",{"v":0.06057692199999999,"d":"0.06"},{"v":0.44268905735280517,"d":"0.44"},{"v":0.44268905735280517,"d":"0.44"},{"v":0.14334724149999997,"d":"0.14"}]
["38025","Dunn","ND",{"v":0.06066133299999999,"d":"0.06"},{"v":0.43874338843831906,"d":"0.44"},{"v":0.43874338843831906,"d":"0.44"},{"v":0.14431274400000002,"d":"0.14"}]
["38027","Eddy","ND",{"v":0.060156248999999995,"d":"0.06"},{"v":0.4302768235875093,"d":"0.43"},{"v":0.43027682358750924,"d":"0.43"},{"v":0.143380529,"d":"0.14"}]
["38029","Emmons","ND",{"v":0.06124867500000001,"d":"0.06"},{"v":0.43176572814115555,"d":"0.43"},{"v":0.43176572814115555,"d":"0.43"},{"v":0.14088043749999998,"d":"0.14"}]
["38031","Foster","ND",{"v":0.06085638200000001,"d":"0.06"},{"v":0.4353369130099854,"d":"0.44"},{"v":0.4353369130099854,"d":"0.44"},{"v":0.14303478249999999,"d":"0.14"}]
["38033","Golden Valley","ND",{"v":0.060780295000000005,"d":"0.06"},{"v":0.41461365966373515,"d":"0.41"},{"v":0.4146136596637351,"d":"0.41"},{"v":0.141232343,"d":"0.14"}]
["38035","Grand Forks","ND",{"v":0.044254013,"d":"0.04"},{"v":0.428802864984119,"d":"0.43"},{"v":0.428802864984119,"d":"0.43"},{"v":0.11991451550000003,"d":"0.12"}]
["38037","Grant","ND",{"v":0.061862481,"d":"0.06"},{"v":0.43381724083953765,"d":"0.43"},{"v":0.43381724083953765,"d":"0.43"},{"v":0.1412178275,"d":"0.14"}]
["38039","Griggs","ND",{"v":0.060915097999999994,"d":"0.06"},{"v":0.4380387278665713,"d":"0.44"},{"v":0.4380387278665713,"d":"0.44"},{"v":0.142450827,"d":"0.14"}]
["38041","Hettinger","ND",{"v":0.061427662,"d":"0.06"},{"v":0.41971608271354666,"d":"0.42"},{"v":0.4197160827135466,"d":"0.42"},{"v":0.140158613,"d":"0.14"}]
["38043","Kidder","ND",{"v":0.06067529099999999,"d":"0.06"},{"v":0.4370613103873412,"d":"0.44"},{"v":0.4370613103873412,"d":"0.44"},{"v":0.1435844755,"d":"0.14"}]
["38045","Lamoure","ND",{"v":0.061464841000000006,"d":"0.06"},{"v":0.43284258407567855,"d":"0.43"},{"v":0.43284258407567866,"d":"0.43"},{"v":0.14070994549999996,"d":"0.14"}]
["38047","Logan","ND",{"v":0.06174312900000001,"d":"0.06"},{"v":0.43366130901131583,"d":"0.43"},{"v":0.4336613090113157,"d":"0.43"},{"v":0.1404513515,"d":"0.14"}]
["38049","McHenry","ND",{"v":0.059831863,"d":"0.06"},{"v":0.4459289524492856,"d":"0.45"},{"v":0.44592895244928565,"d":"0.45"},{"v":0.1450682175,"d":"0.15"}]
["38051","McIntosh","ND",{"v":0.061968258,"d":"0.06"},{"v":0.4312611533333027,"d":"0.43"},{"v":0.43126115333330267,"d":"0.43"},{"v":0.14068253,"d":"0.14"}]
["38053","Mckenzie","ND",{"v":0.058748403,"d":"0.06"},{"v":0.43254976275101165,"d":"0.43"},{"v":0.4325497627510117,"d":"0.43"},{"v":0.143306965,"d":"0.14"}]
["38055","Mclean","ND",{"v":0.060857607,"d":"0.06"},{"v":0.4297925055685305,"d":"0.43"},{"v":0.42979250556853044,"d":"0.43"},{"v":0.1414114085,"d":"0.14"}]
["38057","Mercer","ND",{"v":0.05526461699999999,"d":"0.06"},{"v":0.43353716668847814,"d":"0.43"},{"v":0.43353716668847814,"d":"0.43"},{"v":0.133944809,"d":"0.13"}]
["38059","Morton","ND",{"v":0.050576611,"d":"0.05"},{"v":0.41952686562464225,"d":"0.42"},{"v":0.41952686562464225,"d":"0.42"},{"v":0.123243671,"d":"0.12"}]
["38061","Mountrail","ND",{"v":0.059155137999999996,"d":"0.06"},{"v":0.4470226923769579,"d":"0.45"},{"v":0.4470226923769579,"d":"0.45"},{"v":0.14588182800000002,"d":"0.15"}]
["38063","Nelson","ND",{"v":0.06005034699999999,"d":"0.06"},{"v":0.4448185427450261,"d":"0.44"},{"v":0.4448185427450261,"d":"0.44"},{"v":0.14481763949999998,"d":"0.14"}]
["38065","Oliver","ND",{"v":0.06117051099999999,"d":"0.06"},{"v":0.4342533490397793,"d":"0.43"},{"v":0.43425334903977925,"d":"0.43"},{"v":0.14210701199999998,"d":"0.14"}]
["38067","Pembina","ND",{"v":0.060083202999999995,"d":"0.06"},{"v":0.44585076510641986,"d":"0.45"},{"v":0.44585076510641986,"d":"0.45"},{"v":0.14620984150000002,"d":"0.15"}]
["38069","Pierce","ND",{"v":0.050173957000000005,"d":"0.05"},{"v":0.43493877824593297,"d":"0.43"},{"v":0.43493877824593297,"d":"0.43"},{"v":0.1272352145,"d":"0.13"}]
["38071","Ramsey","ND",{"v":0.048745407,"d":"0.05"},{"v":0.4331909969288614,"d":"0.43"},{"v":0.4331909969288615,"d":"0.43"},{"v":0.1269807895,"d":"0.13"}]
["38073","Ransom","ND",{"v":0.059450393000000004,"d":"0.06"},{"v":0.4306648423519878,"d":"0.43"},{"v":0.43066484235198776,"d":"0.43"},{"v":0.14195146150000001,"d":"0.14"}]
["38075","Renville","ND",{"v":0.061708232999999994,"d":"0.06"},{"v":0.4413912728654627,"d":"0.44"},{"v":0.4413912728654627,"d":"0.44"},{"v":0.1442248015,"d":"0.14"}]
["38077","Richland","ND",{"v":0.052160325,"d":"0.05"},{"v":0.4287926582184186,"d":"0.43"},{"v":0.4287926582184186,"d":"0.43"},{"v":0.13000508,"d":"0.13"}]
["38079","Rolette","ND",{"v":0.05838197800000001,"d":"0.06"},{"v":0.4474435184689762,"d":"0.45"},{"v":0.4474435184689761,"d":"0.45"},{"v":0.14914381200000001,"d":"0.15"}]
["38081","Sargent","ND",{"v":0.061573063000000004,"d":"0.06"},{"v":0.4341536732739916,"d":"0.43"},{"v":0.43415367327399157,"d":"0.43"},{"v":0.1411776135,"d":"0.14"}]
["38083","Sheridan","ND",{"v":0.06012109400000001,"d":"0.06"},{"v":0.44107988327699116,"d":"0.44"},{"v":0.4410798832769912,"d":"0.44"},{"v":0.142918207,"d":"0.14"}]
["38085","Sioux","ND",{"v":0.061437979,"d":"0.06"},{"v":0.4305779140747465,"d":"0.43"},{"v":0.43057791407474655,"d":"0.43"},{"v":0.14145466050000002,"d":"0.14"}]
["38087","Slope","ND",{"v":0.061800931999999996,"d":"0.06"},{"v":0.43055128838502604,"d":"0.43"},{"v":0.43055128838502604,"d":"0.43"},{"v":0.1407128045,"d":"0.14"}]
["38089","Stark","ND",{"v":0.049709756,"d":"0.05"},{"v":0.4165041804764949,"d":"0.42"},{"v":0.4165041804764949,"d":"0.42"},{"v":0.12058946049999998,"d":"0.12"}]
["38091","Steele","ND",{"v":0.060991582,"d":"0.06"},{"v":0.43744935381853844,"d":"0.44"},{"v":0.4374493538185384,"d":"0.44"},{"v":0.143020527,"d":"0.14"}]
["38093","Stutsman","ND",{"v":0.048913537,"d":"0.05"},{"v":0.42711619650106497,"d":"0.43"},{"v":0.42711619650106497,"d":"0.43"},{"v":0.123655153,"d":"0.12"}]
["38095","Towner","ND",{"v":0.059034016,"d":"0.06"},{"v":0.44366482461410744,"d":"0.44"},{"v":0.44366482461410744,"d":"0.44"},{"v":0.14406288650000001,"d":"0.14"}]
["38097","Traill","ND",{"v":0.060322327,"d":"0.06"},{"v":0.4358790910291708,"d":"0.44"},{"v":0.4358790910291708,"d":"0.44"},{"v":0.1429345025,"d":"0.14"}]
["38099","Walsh","ND",{"v":0.05472053599999999,"d":"0.05"},{"v":0.4374750193054444,"d":"0.44"},{"v":0.43747501930544447,"d":"0.44"},{"v":0.13745360049999997,"d":"0.14"}]
["38101","Ward","ND",{"v":0.049514323,"d":"0.05"},{"v":0.42529833004328005,"d":"0.43"},{"v":0.4252983300432801,"d":"0.43"},{"v":0.1215310515,"d":"0.12"}]
["38103","Wells","ND",{"v":0.05992703,"d":"0.06"},{"v":0.43901888199349426,"d":"0.44"},{"v":0.43901888199349426,"d":"0.44"},{"v":0.14332702749999998,"d":"0.14"}]
["38105","Williams","ND",{"v":0.045923777,"d":"0.05"},{"v":0.43322785311978035,"d":"0.43"},{"v":0.4332278531197804,"d":"0.43"},{"v":0.12599701800000002,"d":"0.13"}]
["39001","Adams","OH",{"v":0.360536717,"d":"0.36"},{"v":2.453518634759273,"d":"2.45"},{"v":2.453518634759273,"d":"2.45"},{"v":1.023729742,"d":"1.02"}]
["39003","Allen","OH",{"v":0.3148122649999999,"d":"0.31"},{"v":2.234549288894367,"d":"2.23"},{"v":2.234549288894367,"d":"2.23"},{"v":0.725728995,"d":"0.73"}]
["39005","Ashland","OH",{"v":0.342553146,"d":"0.34"},{"v":2.304810763445914,"d":"2.30"},{"v":2.304810763445914,"d":"2.30"},{"v":0.8872045765000002,"d":"0.89"}]
["39007","Ashtabula","OH",{"v":0.320370039,"d":"0.32"},{"v":2.2981001329213733,"d":"2.30"},{"v":2.2981001329213733,"d":"2.30"},{"v":0.8913248960000001,"d":"0.89"}]
["39009","Athens","OH",{"v":0.297346272,"d":"0.30"},{"v":2.3287271043897393,"d":"2.33"},{"v":2.3287271043897393,"d":"2.33"},{"v":1.0501815575,"d":"1.05"}]
["39011","Auglaize","OH",{"v":0.345746961,"d":"0.35"},{"v":2.286198419546284,"d":"2.29"},{"v":2.2861984195462846,"d":"2.29"},{"v":0.7511302455000001,"d":"0.75"}]
["39013","Belmont","OH",{"v":0.322486765,"d":"0.32"},{"v":2.2722313475017226,"d":"2.27"},{"v":2.2722313475017226,"d":"2.27"},{"v":0.957043416,"d":"0.96"}]
["39015","Brown","OH",{"v":0.367209611,"d":"0.37"},{"v":2.4094868431686263,"d":"2.41"},{"v":2.4094868431686267,"d":"2.41"},{"v":0.8874219565,"d":"0.89"}]
["39017","Butler","OH",{"v":0.2514501,"d":"0.25"},{"v":1.9847932735773854,"d":"1.98"},{"v":1.9847932735773854,"d":"1.98"},{"v":0.6814012845,"d":"0.68"}]
["39019","Carroll","OH",{"v":0.343185702,"d":"0.34"},{"v":2.426205260436966,"d":"2.43"},{"v":2.4262052604369657,"d":"2.43"},{"v":0.9871831799999998,"d":"0.99"}]
["39021","Champaign","OH",{"v":0.37466613399999993,"d":"0.37"},{"v":2.3459011521371282,"d":"2.35"},{"v":2.345901152137128,"d":"2.35"},{"v":0.8198840095,"d":"0.82"}]
["39023","Clark","OH",{"v":0.306869074,"d":"0.31"},{"v":2.1864008347965114,"d":"2.19"},{"v":2.186400834796511,"d":"2.19"},{"v":0.7247830765000001,"d":"0.72"}]
["39025","Clermont","OH",{"v":0.275458662,"d":"0.28"},{"v":2.274702428733595,"d":"2.27"},{"v":2.274702428733595,"d":"2.27"},{"v":0.8082779920000002,"d":"0.81"}]
["39027","Clinton","OH",{"v":0.36021169000000003,"d":"0.36"},{"v":2.296445172714656,"d":"2.30"},{"v":2.296445172714656,"d":"2.30"},{"v":0.7869535995,"d":"0.79"}]
["39029","Columbiana","OH",{"v":0.311651699,"d":"0.31"},{"v":2.3065037630409355,"d":"2.31"},{"v":2.3065037630409355,"d":"2.31"},{"v":0.9059121140000003,"d":"0.91"}]
["39031","Coshocton","OH",{"v":0.32877946300000005,"d":"0.33"},{"v":2.390024763033525,"d":"2.39"},{"v":2.390024763033525,"d":"2.39"},{"v":1.0003101205,"d":"1.00"}]
["39033","Crawford","OH",{"v":0.33882291,"d":"0.34"},{"v":2.2572467059496346,"d":"2.26"},{"v":2.257246705949635,"d":"2.26"},{"v":0.7616756085,"d":"0.76"}]
["39035","Cuyahoga","OH",{"v":0.12296697000000001,"d":"0.12"},{"v":2.4199669014653277E-3,"d":"0.00"},{"v":2.4199669014653277E-3,"d":"0.00"},{"v":0.58296501,"d":"0.58"}]
["39037","Darke","OH",{"v":0.37635329599999995,"d":"0.38"},{"v":2.321364078899344,"d":"2.32"},{"v":2.321364078899344,"d":"2.32"},{"v":0.78902387,"d":"0.79"}]
["39039","Defiance","OH",{"v":0.347755981,"d":"0.35"},{"v":2.3174640214384623,"d":"2.32"},{"v":2.3174640214384623,"d":"2.32"},{"v":0.7706565204999999,"d":"0.77"}]
["39041","Delaware","OH",{"v":0.299187386,"d":"0.30"},{"v":2.18396300806255,"d":"2.18"},{"v":2.18396300806255,"d":"2.18"},{"v":0.717114422,"d":"0.72"}]
["39043","Erie","OH",{"v":0.308775568,"d":"0.31"},{"v":2.218704414107072,"d":"2.22"},{"v":2.218704414107072,"d":"2.22"},{"v":0.7277751919999998,"d":"0.73"}]
["39045","Fairfield","OH",{"v":0.30990924,"d":"0.31"},{"v":2.220043214214589,"d":"2.22"},{"v":2.2200432142145887,"d":"2.22"},{"v":0.7947389850000001,"d":"0.79"}]
["39047","Fayette","OH",{"v":0.364143184,"d":"0.36"},{"v":2.261202910725775,"d":"2.26"},{"v":2.261202910725775,"d":"2.26"},{"v":0.758024549,"d":"0.76"}]
["39049","Franklin","OH",{"v":0.152877957,"d":"0.15"},{"v":0.0281275437716161,"d":"0.03"},{"v":0.0281275437716161,"d":"0.03"},{"v":0.5617708425,"d":"0.56"}]
["39051","Fulton","OH",{"v":0.36173941699999995,"d":"0.36"},{"v":2.299264952970204,"d":"2.30"},{"v":2.299264952970204,"d":"2.30"},{"v":0.7837247645,"d":"0.78"}]
["39053","Gallia","OH",{"v":0.351796771,"d":"0.35"},{"v":2.4054274764060932,"d":"2.41"},{"v":2.405427476406093,"d":"2.41"},{"v":1.0208910539999998,"d":"1.02"}]
["39055","Geauga","OH",{"v":0.32134011700000004,"d":"0.32"},{"v":2.3323792601275475,"d":"2.33"},{"v":2.3323792601275475,"d":"2.33"},{"v":0.9562368199999999,"d":"0.96"}]
["39057","Greene","OH",{"v":0.291994328,"d":"0.29"},{"v":2.1547100235196677,"d":"2.15"},{"v":2.1547100235196677,"d":"2.15"},{"v":0.70207955,"d":"0.70"}]
["39059","Guernsey","OH",{"v":0.329782367,"d":"0.33"},{"v":2.3387777667132346,"d":"2.34"},{"v":2.3387777667132346,"d":"2.34"},{"v":0.9864749864999999,"d":"0.99"}]
["39061","Hamilton","OH",{"v":0.158412095,"d":"0.16"},{"v":0.0736448285216221,"d":"0.07"},{"v":0.0736448285216221,"d":"0.07"},{"v":0.6669522249999998,"d":"0.67"}]
["39063","Hancock","OH",{"v":0.33021291999999997,"d":"0.33"},{"v":2.2339601904282045,"d":"2.23"},{"v":2.2339601904282045,"d":"2.23"},{"v":0.7320144375000002,"d":"0.73"}]
["39065","Hardin","OH",{"v":0.364334089,"d":"0.36"},{"v":2.301636893671353,"d":"2.30"},{"v":2.301636893671353,"d":"2.30"},{"v":0.7895845395,"d":"0.79"}]
["39067","Harrison","OH",{"v":0.357676172,"d":"0.36"},{"v":2.4292614639963284,"d":"2.43"},{"v":2.429261463996329,"d":"2.43"},{"v":1.0315216319999998,"d":"1.03"}]
["39069","Henry","OH",{"v":0.37727112100000004,"d":"0.38"},{"v":2.3144189427840804,"d":"2.31"},{"v":2.31441894278408,"d":"2.31"},{"v":0.7917819809999997,"d":"0.79"}]
["39071","Highland","OH",{"v":0.3691868240000001,"d":"0.37"},{"v":2.3511562610991406,"d":"2.35"},{"v":2.351156261099141,"d":"2.35"},{"v":0.8712843380000002,"d":"0.87"}]
["39073","Hocking","OH",{"v":0.3262875170000001,"d":"0.33"},{"v":2.411786282272367,"d":"2.41"},{"v":2.411786282272367,"d":"2.41"},{"v":1.1414235875000003,"d":"1.14"}]
["39075","Holmes","OH",{"v":0.371411086,"d":"0.37"},{"v":2.359864998530697,"d":"2.36"},{"v":2.359864998530697,"d":"2.36"},{"v":0.9595935135000001,"d":"0.96"}]
["39077","Huron","OH",{"v":0.343745995,"d":"0.34"},{"v":2.2872442135850695,"d":"2.29"},{"v":2.2872442135850695,"d":"2.29"},{"v":0.8226092284999998,"d":"0.82"}]
["39079","Jackson","OH",{"v":0.329284901,"d":"0.33"},{"v":2.3291291742885254,"d":"2.33"},{"v":2.3291291742885254,"d":"2.33"},{"v":1.0233661849999998,"d":"1.02"}]
["39081","Jefferson","OH",{"v":0.29907566399999996,"d":"0.30"},{"v":2.3234287992758453,"d":"2.32"},{"v":2.3234287992758453,"d":"2.32"},{"v":0.9795064320000001,"d":"0.98"}]
["39083","Knox","OH",{"v":0.341708463,"d":"0.34"},{"v":2.3122535070999057,"d":"2.31"},{"v":2.3122535070999057,"d":"2.31"},{"v":0.8947691790000002,"d":"0.89"}]
["39085","Lake","OH",{"v":0.226115157,"d":"0.23"},{"v":1.5570235596964648,"d":"1.56"},{"v":1.5570235596964648,"d":"1.56"},{"v":0.6942889055,"d":"0.69"}]
["39087","Lawrence","OH",{"v":0.305799373,"d":"0.31"},{"v":2.3213123861789335,"d":"2.32"},{"v":2.3213123861789335,"d":"2.32"},{"v":1.038782306,"d":"1.04"}]
["39089","Licking","OH",{"v":0.31356802899999997,"d":"0.31"},{"v":2.2252883981062,"d":"2.23"},{"v":2.2252883981062,"d":"2.23"},{"v":0.8329060765,"d":"0.83"}]
["39091","Logan","OH",{"v":0.354865801,"d":"0.35"},{"v":2.32784150693178,"d":"2.33"},{"v":2.32784150693178,"d":"2.33"},{"v":0.814942625,"d":"0.81"}]
["39093","Lorain","OH",{"v":0.264510763,"d":"0.26"},{"v":2.0985084950607478,"d":"2.10"},{"v":2.098508495060748,"d":"2.10"},{"v":0.7199402330000001,"d":"0.72"}]
["39095","Lucas","OH",{"v":0.208776536,"d":"0.21"},{"v":0.9604780232323193,"d":"0.96"},{"v":0.9604780232323193,"d":"0.96"},{"v":0.6291884135,"d":"0.63"}]
["39097","Madison","OH",{"v":0.36950117499999996,"d":"0.37"},{"v":2.259259011722782,"d":"2.26"},{"v":2.259259011722782,"d":"2.26"},{"v":0.7654882340000001,"d":"0.77"}]
["39099","Mahoning","OH",{"v":0.261474002,"d":"0.26"},{"v":2.0619562162369816,"d":"2.06"},{"v":2.061956216236981,"d":"2.06"},{"v":0.7745638145,"d":"0.77"}]
["39101","Marion","OH",{"v":0.334745432,"d":"0.33"},{"v":2.20350560876477,"d":"2.20"},{"v":2.2035056087647695,"d":"2.20"},{"v":0.7348681380000001,"d":"0.73"}]
["39103","Medina","OH",{"v":0.290053882,"d":"0.29"},{"v":2.22277497081353,"d":"2.22"},{"v":2.2227749708135303,"d":"2.22"},{"v":0.8087942425,"d":"0.81"}]
["39105","Meigs","OH",{"v":0.345223623,"d":"0.35"},{"v":2.4125275285684604,"d":"2.41"},{"v":2.412527528568461,"d":"2.41"},{"v":1.054919372,"d":"1.05"}]
["39107","Mercer","OH",{"v":0.369689735,"d":"0.37"},{"v":2.3001497679147906,"d":"2.30"},{"v":2.30014976791479,"d":"2.30"},{"v":0.7766155134999999,"d":"0.78"}]
["39109","Miami","OH",{"v":0.327130181,"d":"0.33"},{"v":2.2466767864692594,"d":"2.25"},{"v":2.2466767864692594,"d":"2.25"},{"v":0.7331213424999999,"d":"0.73"}]
["39111","Monroe","OH",{"v":0.358249995,"d":"0.36"},{"v":2.309541188587923,"d":"2.31"},{"v":2.3095411885879233,"d":"2.31"},{"v":1.1352239155000001,"d":"1.14"}]
["39113","Montgomery","OH",{"v":0.225088298,"d":"0.23"},{"v":1.18020863323391,"d":"1.18"},{"v":1.18020863323391,"d":"1.18"},{"v":0.6387914805,"d":"0.64"}]
["39115","Morgan","OH",{"v":0.34977776099999996,"d":"0.35"},{"v":2.4031577817661347,"d":"2.40"},{"v":2.4031577817661347,"d":"2.40"},{"v":1.0570799105,"d":"1.06"}]
["39117","Morrow","OH",{"v":0.386500355,"d":"0.39"},{"v":2.413282460926039,"d":"2.41"},{"v":2.4132824609260384,"d":"2.41"},{"v":0.8781622484999999,"d":"0.88"}]
["39119","Muskingum","OH",{"v":0.319063978,"d":"0.32"},{"v":2.256818720228457,"d":"2.26"},{"v":2.2568187202284573,"d":"2.26"},{"v":0.9333446515000002,"d":"0.93"}]
["39121","Noble","OH",{"v":0.345284596,"d":"0.35"},{"v":2.3364379108384004,"d":"2.34"},{"v":2.3364379108384004,"d":"2.34"},{"v":1.0544470400000001,"d":"1.05"}]
["39123","Ottawa","OH",{"v":0.347877355,"d":"0.35"},{"v":2.2939094870534245,"d":"2.29"},{"v":2.2939094870534245,"d":"2.29"},{"v":0.750339306,"d":"0.75"}]
["39125","Paulding","OH",{"v":0.397052276,"d":"0.40"},{"v":2.3860002183635793,"d":"2.39"},{"v":2.386000218363579,"d":"2.39"},{"v":0.8122326999999999,"d":"0.81"}]
["39127","Perry","OH",{"v":0.344471873,"d":"0.34"},{"v":2.360258470299153,"d":"2.36"},{"v":2.360258470299153,"d":"2.36"},{"v":1.0019739995000003,"d":"1.00"}]
["39129","Pickaway","OH",{"v":0.36063482099999994,"d":"0.36"},{"v":2.275997674157587,"d":"2.28"},{"v":2.2759976741575874,"d":"2.28"},{"v":0.7771885869999999,"d":"0.78"}]
["39131","Pike","OH",{"v":0.33891303,"d":"0.34"},{"v":2.4309251849416644,"d":"2.43"},{"v":2.430925184941665,"d":"2.43"},{"v":1.0206346765,"d":"1.02"}]
["39133","Portage","OH",{"v":0.292685145,"d":"0.29"},{"v":2.290316575911998,"d":"2.29"},{"v":2.2903165759119974,"d":"2.29"},{"v":0.8516260664999998,"d":"0.85"}]
["39135","Preble","OH",{"v":0.37552601300000005,"d":"0.38"},{"v":2.304032999855289,"d":"2.30"},{"v":2.3040329998552886,"d":"2.30"},{"v":0.8103434660000001,"d":"0.81"}]
["39137","Putnam","OH",{"v":0.398213841,"d":"0.40"},{"v":2.3802109498450807,"d":"2.38"},{"v":2.3802109498450816,"d":"2.38"},{"v":0.8093237355000001,"d":"0.81"}]
["39139","Richland","OH",{"v":0.30599182900000005,"d":"0.31"},{"v":2.233561341999342,"d":"2.23"},{"v":2.233561341999342,"d":"2.23"},{"v":0.8273927040000002,"d":"0.83"}]
["39141","Ross","OH",{"v":0.33983075599999996,"d":"0.34"},{"v":2.314023009051408,"d":"2.31"},{"v":2.314023009051408,"d":"2.31"},{"v":0.9176658619999998,"d":"0.92"}]
["39143","Sandusky","OH",{"v":0.34614691700000005,"d":"0.35"},{"v":2.2514160830081034,"d":"2.25"},{"v":2.251416083008104,"d":"2.25"},{"v":0.7612787679999998,"d":"0.76"}]
["39145","Scioto","OH",{"v":0.313836167,"d":"0.31"},{"v":2.3126355819220383,"d":"2.31"},{"v":2.3126355819220383,"d":"2.31"},{"v":1.0252002544999999,"d":"1.03"}]
["39147","Seneca","OH",{"v":0.352988512,"d":"0.35"},{"v":2.288338313118567,"d":"2.29"},{"v":2.2883383131185675,"d":"2.29"},{"v":0.7752348769999999,"d":"0.78"}]
["39149","Shelby","OH",{"v":0.35453074000000007,"d":"0.35"},{"v":2.2655478503067,"d":"2.27"},{"v":2.2655478503066995,"d":"2.27"},{"v":0.7833569104999999,"d":"0.78"}]
["39151","Stark","OH",{"v":0.257605676,"d":"0.26"},{"v":1.9866696564728141,"d":"1.99"},{"v":1.986669656472814,"d":"1.99"},{"v":0.738365676,"d":"0.74"}]
["39153","Summit","OH",{"v":0.19760505899999997,"d":"0.20"},{"v":0.8745391246686778,"d":"0.87"},{"v":0.8745391246686777,"d":"0.87"},{"v":0.7158540085,"d":"0.72"}]
["39155","Trumbull","OH",{"v":0.285779944,"d":"0.29"},{"v":2.180449391954437,"d":"2.18"},{"v":2.1804493919544368,"d":"2.18"},{"v":0.844266755,"d":"0.84"}]
["39157","Tuscarawas","OH",{"v":0.312176532,"d":"0.31"},{"v":2.2549044802787317,"d":"2.25"},{"v":2.2549044802787317,"d":"2.25"},{"v":0.9251890395000001,"d":"0.93"}]
["39159","Union","OH",{"v":0.359952552,"d":"0.36"},{"v":2.279256853163734,"d":"2.28"},{"v":2.2792568531637336,"d":"2.28"},{"v":0.7742139039999999,"d":"0.77"}]
["39161","Van Wert","OH",{"v":0.363692678,"d":"0.36"},{"v":2.32220312991381,"d":"2.32"},{"v":2.32220312991381,"d":"2.32"},{"v":0.7603910405000001,"d":"0.76"}]
["39163","Vinton","OH",{"v":0.354979384,"d":"0.35"},{"v":2.535890501674412,"d":"2.54"},{"v":2.535890501674412,"d":"2.54"},{"v":1.1487432255,"d":"1.15"}]
["39165","Warren","OH",{"v":0.278026328,"d":"0.28"},{"v":2.1570306664526897,"d":"2.16"},{"v":2.1570306664526897,"d":"2.16"},{"v":0.7396944370000001,"d":"0.74"}]
["39167","Washington","OH",{"v":0.317236184,"d":"0.32"},{"v":2.2331966844770013,"d":"2.23"},{"v":2.2331966844770017,"d":"2.23"},{"v":1.0292444834999999,"d":"1.03"}]
["39169","Wayne","OH",{"v":0.334233353,"d":"0.33"},{"v":2.2455092145133424,"d":"2.25"},{"v":2.2455092145133424,"d":"2.25"},{"v":0.808199545,"d":"0.81"}]
["39171","Williams","OH",{"v":0.366766844,"d":"0.37"},{"v":2.290505059872357,"d":"2.29"},{"v":2.290505059872357,"d":"2.29"},{"v":0.8102769459999998,"d":"0.81"}]
["39173","Wood","OH",{"v":0.320137993,"d":"0.32"},{"v":2.241605153384145,"d":"2.24"},{"v":2.2416051533841452,"d":"2.24"},{"v":0.7167213765000001,"d":"0.72"}]
["39175","Wyandot","OH",{"v":0.362371069,"d":"0.36"},{"v":2.331610689261922,"d":"2.33"},{"v":2.331610689261922,"d":"2.33"},{"v":0.7932495904999998,"d":"0.79"}]
["40001","Adair","OK",{"v":0.310453514,"d":"0.31"},{"v":1.8101230188538624,"d":"1.81"},{"v":1.8101230188538624,"d":"1.81"},{"v":0.8290302445000001,"d":"0.83"}]
["40003","Alfalfa","OK",{"v":0.36871411400000004,"d":"0.37"},{"v":1.7848182591120738,"d":"1.78"},{"v":1.7848182591120743,"d":"1.78"},{"v":0.6538111480000001,"d":"0.65"}]
["40005","Atoka","OK",{"v":0.332589029,"d":"0.33"},{"v":1.8246094057374063,"d":"1.82"},{"v":1.824609405737406,"d":"1.82"},{"v":0.8090773945,"d":"0.81"}]
["40007","Beaver","OK",{"v":0.367720558,"d":"0.37"},{"v":1.817749453579251,"d":"1.82"},{"v":1.817749453579251,"d":"1.82"},{"v":0.6533671185,"d":"0.65"}]
["40009","Beckham","OK",{"v":0.30879928500000003,"d":"0.31"},{"v":1.7193278159366447,"d":"1.72"},{"v":1.7193278159366447,"d":"1.72"},{"v":0.596991889,"d":"0.60"}]
["40011","Blaine","OK",{"v":0.332673675,"d":"0.33"},{"v":1.7826145785106906,"d":"1.78"},{"v":1.7826145785106906,"d":"1.78"},{"v":0.6467935795,"d":"0.65"}]
["40013","Bryan","OK",{"v":0.311363664,"d":"0.31"},{"v":1.7808976738558295,"d":"1.78"},{"v":1.7808976738558293,"d":"1.78"},{"v":0.6776153690000001,"d":"0.68"}]
["40015","Caddo","OK",{"v":0.34780266000000004,"d":"0.35"},{"v":1.7450603245832945,"d":"1.75"},{"v":1.7450603245832943,"d":"1.75"},{"v":0.649385575,"d":"0.65"}]
["40017","Canadian","OK",{"v":0.28425535500000004,"d":"0.28"},{"v":1.6859264446008342,"d":"1.69"},{"v":1.6859264446008342,"d":"1.69"},{"v":0.5649864664999998,"d":"0.56"}]
["40019","Carter","OK",{"v":0.311416246,"d":"0.31"},{"v":1.7451615117645762,"d":"1.75"},{"v":1.7451615117645762,"d":"1.75"},{"v":0.6632486830000001,"d":"0.66"}]
["40021","Cherokee","OK",{"v":0.286380658,"d":"0.29"},{"v":1.79849601373231,"d":"1.80"},{"v":1.7984960137323103,"d":"1.80"},{"v":0.7867508305,"d":"0.79"}]
["40023","Choctaw","OK",{"v":0.313371313,"d":"0.31"},{"v":1.7934785239990516,"d":"1.79"},{"v":1.7934785239990516,"d":"1.79"},{"v":0.727731151,"d":"0.73"}]
["40025","Cimarron","OK",{"v":0.37082947400000005,"d":"0.37"},{"v":1.7886460744944817,"d":"1.79"},{"v":1.7886460744944817,"d":"1.79"},{"v":0.6514936754999999,"d":"0.65"}]
["40027","Cleveland","OK",{"v":0.23228405699999996,"d":"0.23"},{"v":1.6442246821031496,"d":"1.64"},{"v":1.6442246821031492,"d":"1.64"},{"v":0.613595454,"d":"0.61"}]
["40029","Coal","OK",{"v":0.348929663,"d":"0.35"},{"v":1.7412289773788356,"d":"1.74"},{"v":1.741228977378836,"d":"1.74"},{"v":0.7668729085,"d":"0.77"}]
["40031","Comanche","OK",{"v":0.28416105899999994,"d":"0.28"},{"v":1.6950181375579507,"d":"1.70"},{"v":1.6950181375579507,"d":"1.70"},{"v":0.5635367035,"d":"0.56"}]
["40033","Cotton","OK",{"v":0.335938616,"d":"0.34"},{"v":1.7336887896533617,"d":"1.73"},{"v":1.7336887896533617,"d":"1.73"},{"v":0.6086502945,"d":"0.61"}]
["40035","Craig","OK",{"v":0.32395096400000006,"d":"0.32"},{"v":1.8257914895707328,"d":"1.83"},{"v":1.8257914895707326,"d":"1.83"},{"v":0.644607723,"d":"0.64"}]
["40037","Creek","OK",{"v":0.292353547,"d":"0.29"},{"v":1.7691773837880653,"d":"1.77"},{"v":1.7691773837880653,"d":"1.77"},{"v":0.7221731855,"d":"0.72"}]
["40039","Custer","OK",{"v":0.301167371,"d":"0.30"},{"v":1.7501737253033187,"d":"1.75"},{"v":1.7501737253033185,"d":"1.75"},{"v":0.5832010340000001,"d":"0.58"}]
["40041","Delaware","OK",{"v":0.31396015900000007,"d":"0.31"},{"v":1.9193439900677791,"d":"1.92"},{"v":1.9193439900677791,"d":"1.92"},{"v":0.7701426749999998,"d":"0.77"}]
["40043","Dewey","OK",{"v":0.360809663,"d":"0.36"},{"v":1.807827485278449,"d":"1.81"},{"v":1.807827485278449,"d":"1.81"},{"v":0.6911399085,"d":"0.69"}]
["40045","Ellis","OK",{"v":0.364222034,"d":"0.36"},{"v":1.841481248983157,"d":"1.84"},{"v":1.8414812489831567,"d":"1.84"},{"v":0.6679882370000002,"d":"0.67"}]
["40047","Garfield","OK",{"v":0.294211716,"d":"0.29"},{"v":1.7345193968371868,"d":"1.73"},{"v":1.7345193968371866,"d":"1.73"},{"v":0.5628920885,"d":"0.56"}]
["40049","Garvin","OK",{"v":0.32876886799999994,"d":"0.33"},{"v":1.7744352521208058,"d":"1.77"},{"v":1.7744352521208058,"d":"1.77"},{"v":0.663969173,"d":"0.66"}]
["40051","Grady","OK",{"v":0.32027546,"d":"0.32"},{"v":1.7857250612544457,"d":"1.79"},{"v":1.7857250612544457,"d":"1.79"},{"v":0.6484641990000001,"d":"0.65"}]
["40053","Grant","OK",{"v":0.369329791,"d":"0.37"},{"v":1.7829111245616605,"d":"1.78"},{"v":1.7829111245616605,"d":"1.78"},{"v":0.6525359965,"d":"0.65"}]
["40055","Greer","OK",{"v":0.319630691,"d":"0.32"},{"v":1.6041826203579317,"d":"1.60"},{"v":1.6041826203579321,"d":"1.60"},{"v":0.6021038545,"d":"0.60"}]
["40057","Harmon","OK",{"v":0.379359632,"d":"0.38"},{"v":1.6453267591960063,"d":"1.65"},{"v":1.645326759196006,"d":"1.65"},{"v":0.6461946364999999,"d":"0.65"}]
["40059","Harper","OK",{"v":0.36971078399999996,"d":"0.37"},{"v":1.8136058367498047,"d":"1.81"},{"v":1.8136058367498047,"d":"1.81"},{"v":0.6548791759999999,"d":"0.65"}]
["40061","Haskell","OK",{"v":0.32060341500000006,"d":"0.32"},{"v":1.814288465452994,"d":"1.81"},{"v":1.814288465452994,"d":"1.81"},{"v":0.7353532564999999,"d":"0.74"}]
["40063","Hughes","OK",{"v":0.307594059,"d":"0.31"},{"v":1.801504573454954,"d":"1.80"},{"v":1.801504573454954,"d":"1.80"},{"v":0.7575934835000001,"d":"0.76"}]
["40065","Jackson","OK",{"v":0.304174107,"d":"0.30"},{"v":1.664958623386549,"d":"1.66"},{"v":1.664958623386549,"d":"1.66"},{"v":0.559594228,"d":"0.56"}]
["40067","Jefferson","OK",{"v":0.37057678,"d":"0.37"},{"v":1.6762277285298093,"d":"1.68"},{"v":1.6762277285298093,"d":"1.68"},{"v":0.6621275804999999,"d":"0.66"}]
["40069","Johnston","OK",{"v":0.347335785,"d":"0.35"},{"v":1.802575864242384,"d":"1.80"},{"v":1.8025758642423841,"d":"1.80"},{"v":0.7468397775,"d":"0.75"}]
["40071","Kay","OK",{"v":0.294564058,"d":"0.29"},{"v":1.7100972461452495,"d":"1.71"},{"v":1.7100972461452497,"d":"1.71"},{"v":0.5736671785,"d":"0.57"}]
["40073","Kingfisher","OK",{"v":0.342302207,"d":"0.34"},{"v":1.7560305465336612,"d":"1.76"},{"v":1.7560305465336612,"d":"1.76"},{"v":0.6252261855,"d":"0.63"}]
["40075","Kiowa","OK",{"v":0.344686151,"d":"0.34"},{"v":1.678386036495067,"d":"1.68"},{"v":1.678386036495067,"d":"1.68"},{"v":0.6105270115,"d":"0.61"}]
["40077","Latimer","OK",{"v":0.29990528599999994,"d":"0.30"},{"v":1.8081561302122957,"d":"1.81"},{"v":1.8081561302122955,"d":"1.81"},{"v":0.8603021100000001,"d":"0.86"}]
["40079","Le Flore","OK",{"v":0.299916289,"d":"0.30"},{"v":1.7771876940630766,"d":"1.78"},{"v":1.777187694063077,"d":"1.78"},{"v":0.8476287429999999,"d":"0.85"}]
["40081","Lincoln","OK",{"v":0.338541159,"d":"0.34"},{"v":1.8256552336976077,"d":"1.83"},{"v":1.825655233697608,"d":"1.83"},{"v":0.718034094,"d":"0.72"}]
["40083","Logan","OK",{"v":0.310295517,"d":"0.31"},{"v":1.7755938271136928,"d":"1.78"},{"v":1.7755938271136926,"d":"1.78"},{"v":0.6583910295000001,"d":"0.66"}]
["40085","Love","OK",{"v":0.35124991600000005,"d":"0.35"},{"v":1.8233512929098095,"d":"1.82"},{"v":1.8233512929098095,"d":"1.82"},{"v":0.7309786180000001,"d":"0.73"}]
["40087","Mcclain","OK",{"v":0.329401781,"d":"0.33"},{"v":1.7803407227678396,"d":"1.78"},{"v":1.7803407227678396,"d":"1.78"},{"v":0.6734893005,"d":"0.67"}]
["40089","McCurtain","OK",{"v":0.297149548,"d":"0.30"},{"v":1.8038675232761252,"d":"1.80"},{"v":1.803867523276125,"d":"1.80"},{"v":0.8544801940000002,"d":"0.85"}]
["40091","McIntosh","OK",{"v":0.33161624100000003,"d":"0.33"},{"v":1.8466984769263493,"d":"1.85"},{"v":1.8466984769263493,"d":"1.85"},{"v":0.7216607505000002,"d":"0.72"}]
["40093","Major","OK",{"v":0.360821462,"d":"0.36"},{"v":1.8291502499475103,"d":"1.83"},{"v":1.82915024994751,"d":"1.83"},{"v":0.6809625825,"d":"0.68"}]
["40095","Marshall","OK",{"v":0.32484488,"d":"0.32"},{"v":1.826107267044462,"d":"1.83"},{"v":1.826107267044462,"d":"1.83"},{"v":0.6990788245,"d":"0.70"}]
["40097","Mayes","OK",{"v":0.316764852,"d":"0.32"},{"v":1.8574049052455668,"d":"1.86"},{"v":1.8574049052455668,"d":"1.86"},{"v":0.720315945,"d":"0.72"}]
["40099","Murray","OK",{"v":0.30710470199999995,"d":"0.31"},{"v":1.7698570408374321,"d":"1.77"},{"v":1.7698570408374321,"d":"1.77"},{"v":0.6528626224999999,"d":"0.65"}]
["40101","Muskogee","OK",{"v":0.288681161,"d":"0.29"},{"v":1.7352077680433267,"d":"1.74"},{"v":1.7352077680433267,"d":"1.74"},{"v":0.6467789804999999,"d":"0.65"}]
["40103","Noble","OK",{"v":0.319617293,"d":"0.32"},{"v":1.8215017811756868,"d":"1.82"},{"v":1.8215017811756868,"d":"1.82"},{"v":0.630613055,"d":"0.63"}]
["40105","Nowata","OK",{"v":0.318584495,"d":"0.32"},{"v":1.8056379818961918,"d":"1.81"},{"v":1.805637981896192,"d":"1.81"},{"v":0.6482014945,"d":"0.65"}]
["40107","Okfuskee","OK",{"v":0.318444508,"d":"0.32"},{"v":1.801381396818278,"d":"1.80"},{"v":1.8013813968182777,"d":"1.80"},{"v":0.7300679560000001,"d":"0.73"}]
["40109","Oklahoma","OK",{"v":0.1920799,"d":"0.19"},{"v":1.1673837021050333,"d":"1.17"},{"v":1.1673837021050333,"d":"1.17"},{"v":0.5309058624999999,"d":"0.53"}]
["40111","Okmulgee","OK",{"v":0.298740824,"d":"0.30"},{"v":1.7359835925262506,"d":"1.74"},{"v":1.7359835925262503,"d":"1.74"},{"v":0.6914740315,"d":"0.69"}]
["40113","Osage","OK",{"v":0.320674475,"d":"0.32"},{"v":1.8011764406459896,"d":"1.80"},{"v":1.8011764406459896,"d":"1.80"},{"v":0.6639310749999999,"d":"0.66"}]
["40115","Ottawa","OK",{"v":0.302549984,"d":"0.30"},{"v":1.7889775504006764,"d":"1.79"},{"v":1.7889775504006764,"d":"1.79"},{"v":0.6510760155,"d":"0.65"}]
["40117","Pawnee","OK",{"v":0.326674045,"d":"0.33"},{"v":1.8531273293817603,"d":"1.85"},{"v":1.8531273293817603,"d":"1.85"},{"v":0.7064258505,"d":"0.71"}]
["40119","Payne","OK",{"v":0.27767234200000007,"d":"0.28"},{"v":1.711435883234253,"d":"1.71"},{"v":1.7114358832342533,"d":"1.71"},{"v":0.6262359084999999,"d":"0.63"}]
["40121","Pittsburg","OK",{"v":0.298284578,"d":"0.30"},{"v":1.7699177728187712,"d":"1.77"},{"v":1.7699177728187712,"d":"1.77"},{"v":0.7343105360000001,"d":"0.73"}]
["40123","Pontotoc","OK",{"v":0.30204652000000004,"d":"0.30"},{"v":1.690384088331762,"d":"1.69"},{"v":1.690384088331762,"d":"1.69"},{"v":0.69935121,"d":"0.70"}]
["40125","Pottawatomie","OK",{"v":0.292723655,"d":"0.29"},{"v":1.734075620204513,"d":"1.73"},{"v":1.7340756202045131,"d":"1.73"},{"v":0.6889791115,"d":"0.69"}]
["40127","Pushmataha","OK",{"v":0.319500463,"d":"0.32"},{"v":1.8454180598578456,"d":"1.85"},{"v":1.8454180598578456,"d":"1.85"},{"v":0.910282493,"d":"0.91"}]
["40129","Roger Mills","OK",{"v":0.365738894,"d":"0.37"},{"v":1.8141070364894596,"d":"1.81"},{"v":1.8141070364894598,"d":"1.81"},{"v":0.6653737839999999,"d":"0.67"}]
["40131","Rogers","OK",{"v":0.296889298,"d":"0.30"},{"v":1.7398837615918301,"d":"1.74"},{"v":1.7398837615918301,"d":"1.74"},{"v":0.650552679,"d":"0.65"}]
["40133","Seminole","OK",{"v":0.306964851,"d":"0.31"},{"v":1.7916423314104346,"d":"1.79"},{"v":1.7916423314104346,"d":"1.79"},{"v":0.7397731049999999,"d":"0.74"}]
["40135","Sequoyah","OK",{"v":0.30140914,"d":"0.30"},{"v":1.8242330490266323,"d":"1.82"},{"v":1.8242330490266323,"d":"1.82"},{"v":0.754469716,"d":"0.75"}]
["40137","Stephens","OK",{"v":0.307479652,"d":"0.31"},{"v":1.6974105984150991,"d":"1.70"},{"v":1.6974105984150991,"d":"1.70"},{"v":0.6288450389999999,"d":"0.63"}]
["40139","Texas","OK",{"v":0.315733406,"d":"0.32"},{"v":1.8055545528839358,"d":"1.81"},{"v":1.805554552883936,"d":"1.81"},{"v":0.595991271,"d":"0.60"}]
["40141","Tillman","OK",{"v":0.332109234,"d":"0.33"},{"v":1.6557325563711813,"d":"1.66"},{"v":1.6557325563711816,"d":"1.66"},{"v":0.5917664669999999,"d":"0.59"}]
["40143","Tulsa","OK",{"v":0.18655433699999996,"d":"0.19"},{"v":1.1121525404726447,"d":"1.11"},{"v":1.1121525404726444,"d":"1.11"},{"v":0.530715647,"d":"0.53"}]
["40145","Wagoner","OK",{"v":0.28726307599999995,"d":"0.29"},{"v":1.7517765371336351,"d":"1.75"},{"v":1.7517765371336353,"d":"1.75"},{"v":0.640182878,"d":"0.64"}]
["40147","Washington","OK",{"v":0.2783515650000001,"d":"0.28"},{"v":1.7073590585944607,"d":"1.71"},{"v":1.7073590585944607,"d":"1.71"},{"v":0.6027245995,"d":"0.60"}]
["40149","Washita","OK",{"v":0.35470297900000003,"d":"0.35"},{"v":1.76150667738156,"d":"1.76"},{"v":1.7615066773815602,"d":"1.76"},{"v":0.6259919090000001,"d":"0.63"}]
["40151","Woods","OK",{"v":0.306801513,"d":"0.31"},{"v":1.7326191079649178,"d":"1.73"},{"v":1.7326191079649178,"d":"1.73"},{"v":0.5979999455000001,"d":"0.60"}]
["40153","Woodward","OK",{"v":0.303596815,"d":"0.30"},{"v":1.8055246960660674,"d":"1.81"},{"v":1.8055246960660674,"d":"1.81"},{"v":0.6147628245,"d":"0.61"}]
["41001","Baker","OR",{"v":0.606587789,"d":"0.61"},{"v":4.583186896356017,"d":"4.58"},{"v":4.5831868963560165,"d":"4.58"},{"v":1.5098281049999998,"d":"1.51"}]
["41003","Benton","OR",{"v":0.5318921519999998,"d":"0.53"},{"v":4.025968875650542,"d":"4.03"},{"v":4.025968875650542,"d":"4.03"},{"v":1.5766641010000002,"d":"1.58"}]
["41005","Clackamas","OR",{"v":0.507127503,"d":"0.51"},{"v":4.021476703597941,"d":"4.02"},{"v":4.021476703597941,"d":"4.02"},{"v":1.653798898,"d":"1.65"}]
["41007","Clatsop","OR",{"v":0.586018495,"d":"0.59"},{"v":3.9726885813708765,"d":"3.97"},{"v":3.9726885813708765,"d":"3.97"},{"v":1.651311087,"d":"1.65"}]
["41009","Columbia","OR",{"v":0.5751493799999999,"d":"0.58"},{"v":4.128847618854366,"d":"4.13"},{"v":4.128847618854367,"d":"4.13"},{"v":1.768617133,"d":"1.77"}]
["41011","Coos","OR",{"v":0.5810854539999999,"d":"0.58"},{"v":4.2873416130157285,"d":"4.29"},{"v":4.2873416130157285,"d":"4.29"},{"v":1.6888451154999997,"d":"1.69"}]
["41013","Crook","OR",{"v":0.6297294860000001,"d":"0.63"},{"v":4.560731103282424,"d":"4.56"},{"v":4.560731103282424,"d":"4.56"},{"v":1.4845807605,"d":"1.48"}]
["41015","Curry","OR",{"v":0.586328709,"d":"0.59"},{"v":4.318834624462319,"d":"4.32"},{"v":4.318834624462319,"d":"4.32"},{"v":1.7088456074999998,"d":"1.71"}]
["41017","Deschutes","OR",{"v":0.579470682,"d":"0.58"},{"v":4.477570897202147,"d":"4.48"},{"v":4.477570897202147,"d":"4.48"},{"v":1.5021213905,"d":"1.50"}]
["41019","Douglas","OR",{"v":0.572238905,"d":"0.57"},{"v":4.364428964312487,"d":"4.36"},{"v":4.364428964312488,"d":"4.36"},{"v":1.8072506185000001,"d":"1.81"}]
["41021","Gilliam","OR",{"v":0.7702198360000001,"d":"0.77"},{"v":4.341573411016517,"d":"4.34"},{"v":4.341573411016517,"d":"4.34"},{"v":1.4621241234999998,"d":"1.46"}]
["41023","Grant","OR",{"v":0.68852909,"d":"0.69"},{"v":4.795618836247647,"d":"4.80"},{"v":4.795618836247647,"d":"4.80"},{"v":1.7489997094999996,"d":"1.75"}]
["41025","Harney","OR",{"v":0.6336263670000001,"d":"0.63"},{"v":4.549225140627909,"d":"4.55"},{"v":4.549225140627909,"d":"4.55"},{"v":1.4101456625,"d":"1.41"}]
["41027","Hood River","OR",{"v":0.5636782560000001,"d":"0.56"},{"v":4.364199543952513,"d":"4.36"},{"v":4.364199543952513,"d":"4.36"},{"v":1.8535548405,"d":"1.85"}]
["41029","Jackson","OR",{"v":0.5491103089999999,"d":"0.55"},{"v":4.232018221225496,"d":"4.23"},{"v":4.232018221225496,"d":"4.23"},{"v":1.6655143290000005,"d":"1.67"}]
["41031","Jefferson","OR",{"v":0.6469064759999998,"d":"0.65"},{"v":4.651660022363356,"d":"4.65"},{"v":4.651660022363355,"d":"4.65"},{"v":1.5620412774999999,"d":"1.56"}]
["41033","Josephine","OR",{"v":0.569382049,"d":"0.57"},{"v":4.298359383517786,"d":"4.30"},{"v":4.298359383517786,"d":"4.30"},{"v":1.8515406514999997,"d":"1.85"}]
["41035","Klamath","OR",{"v":0.587311278,"d":"0.59"},{"v":4.599069689660777,"d":"4.60"},{"v":4.599069689660777,"d":"4.60"},{"v":1.6281419825,"d":"1.63"}]
["41037","Lake","OR",{"v":0.655914512,"d":"0.66"},{"v":4.61318351049432,"d":"4.61"},{"v":4.61318351049432,"d":"4.61"},{"v":1.520956121,"d":"1.52"}]
["41039","Lane","OR",{"v":0.531438865,"d":"0.53"},{"v":4.22622409697175,"d":"4.23"},{"v":4.22622409697175,"d":"4.23"},{"v":1.6812596184999997,"d":"1.68"}]
["41041","Lincoln","OR",{"v":0.5826365150000001,"d":"0.58"},{"v":4.171403674261842,"d":"4.17"},{"v":4.171403674261842,"d":"4.17"},{"v":1.6728776565,"d":"1.67"}]
["41043","Linn","OR",{"v":0.575558032,"d":"0.58"},{"v":4.086350080139374,"d":"4.09"},{"v":4.086350080139374,"d":"4.09"},{"v":1.6319611609999995,"d":"1.63"}]
["41045","Malheur","OR",{"v":0.647091541,"d":"0.65"},{"v":4.297700341476816,"d":"4.30"},{"v":4.297700341476815,"d":"4.30"},{"v":1.3666516565000002,"d":"1.37"}]
["41047","Marion","OR",{"v":0.514455346,"d":"0.51"},{"v":3.973929915677602,"d":"3.97"},{"v":3.973929915677602,"d":"3.97"},{"v":1.4604172439999996,"d":"1.46"}]
["41049","Morrow","OR",{"v":0.662114471,"d":"0.66"},{"v":4.362585442144137,"d":"4.36"},{"v":4.362585442144137,"d":"4.36"},{"v":1.4038169639999998,"d":"1.40"}]
["41051","Multnomah","OR",{"v":0.294405942,"d":"0.29"},{"v":0.32845910897156294,"d":"0.33"},{"v":0.32845910897156294,"d":"0.33"},{"v":1.2425903464999999,"d":"1.24"}]
["41053","Polk","OR",{"v":0.5574538979999999,"d":"0.56"},{"v":4.057493253633476,"d":"4.06"},{"v":4.057493253633476,"d":"4.06"},{"v":1.5401474275000002,"d":"1.54"}]
["41055","Sherman","OR",{"v":0.769879041,"d":"0.77"},{"v":4.388674031220644,"d":"4.39"},{"v":4.388674031220644,"d":"4.39"},{"v":1.4631009349999997,"d":"1.46"}]
["41057","Tillamook","OR",{"v":0.64381147,"d":"0.64"},{"v":4.2931795593850435,"d":"4.29"},{"v":4.2931795593850435,"d":"4.29"},{"v":1.7663752415000002,"d":"1.77"}]
["41059","Umatilla","OR",{"v":0.615351399,"d":"0.62"},{"v":4.2210492482087965,"d":"4.22"},{"v":4.2210492482087965,"d":"4.22"},{"v":1.3545848415000001,"d":"1.35"}]
["41061","Union","OR",{"v":0.5801409439999999,"d":"0.58"},{"v":4.574222100672131,"d":"4.57"},{"v":4.574222100672131,"d":"4.57"},{"v":1.6265858965,"d":"1.63"}]
["41063","Wallowa","OR",{"v":0.698137757,"d":"0.70"},{"v":4.79228844151063,"d":"4.79"},{"v":4.79228844151063,"d":"4.79"},{"v":1.7128935230000006,"d":"1.71"}]
["41065","Wasco","OR",{"v":0.618137283,"d":"0.62"},{"v":4.331186177808337,"d":"4.33"},{"v":4.331186177808337,"d":"4.33"},{"v":1.4168858290000002,"d":"1.42"}]
["41067","Washington","OR",{"v":0.424844481,"d":"0.42"},{"v":3.5515620024020675,"d":"3.55"},{"v":3.5515620024020675,"d":"3.55"},{"v":1.3898080375,"d":"1.39"}]
["41069","Wheeler","OR",{"v":0.72191936,"d":"0.72"},{"v":4.698344963891786,"d":"4.70"},{"v":4.698344963891785,"d":"4.70"},{"v":1.6255774765000002,"d":"1.63"}]
["41071","Yamhill","OR",{"v":0.555069304,"d":"0.56"},{"v":4.157920204080287,"d":"4.16"},{"v":4.157920204080288,"d":"4.16"},{"v":1.5529393194999999,"d":"1.55"}]
["42001","Adams","PA",{"v":0.289582445,"d":"0.29"},{"v":1.9968875655183744,"d":"2.00"},{"v":1.9968875655183744,"d":"2.00"},{"v":0.7546303690000001,"d":"0.75"}]
["42003","Allegheny","PA",{"v":0.14865717399999998,"d":"0.15"},{"v":0.16412148277081604,"d":"0.16"},{"v":0.16412148277081604,"d":"0.16"},{"v":0.626581083,"d":"0.63"}]
["42005","Armstrong","PA",{"v":0.281691605,"d":"0.28"},{"v":1.9440043125458275,"d":"1.94"},{"v":1.9440043125458277,"d":"1.94"},{"v":0.8781088519999999,"d":"0.88"}]
["42007","Beaver","PA",{"v":0.236015775,"d":"0.24"},{"v":1.8931725971667177,"d":"1.89"},{"v":1.8931725971667177,"d":"1.89"},{"v":0.7707257955000002,"d":"0.77"}]
["42009","Bedford","PA",{"v":0.28801131,"d":"0.29"},{"v":2.2139039049345266,"d":"2.21"},{"v":2.2139039049345266,"d":"2.21"},{"v":0.9614124485000001,"d":"0.96"}]
["42011","Berks","PA",{"v":0.26438420799999995,"d":"0.26"},{"v":1.9501838259611428,"d":"1.95"},{"v":1.9501838259611433,"d":"1.95"},{"v":0.6819289635,"d":"0.68"}]
["42013","Blair","PA",{"v":0.23400726299999997,"d":"0.23"},{"v":1.9802977135867363,"d":"1.98"},{"v":1.9802977135867363,"d":"1.98"},{"v":0.849722706,"d":"0.85"}]
["42015","Bradford","PA",{"v":0.284893474,"d":"0.28"},{"v":2.1960105766124927,"d":"2.20"},{"v":2.1960105766124927,"d":"2.20"},{"v":0.8817906884999999,"d":"0.88"}]
["42017","Bucks","PA",{"v":0.20175742199999996,"d":"0.20"},{"v":1.4759946406002349,"d":"1.48"},{"v":1.4759946406002353,"d":"1.48"},{"v":0.6127592225,"d":"0.61"}]
["42019","Butler","PA",{"v":0.2612476879999999,"d":"0.26"},{"v":1.9774588350251894,"d":"1.98"},{"v":1.9774588350251896,"d":"1.98"},{"v":0.793837511,"d":"0.79"}]
["42021","Cambria","PA",{"v":0.247959389,"d":"0.25"},{"v":2.0481853746587566,"d":"2.05"},{"v":2.048185374658757,"d":"2.05"},{"v":0.8737816319999999,"d":"0.87"}]
["42023","Cameron","PA",{"v":0.255729463,"d":"0.26"},{"v":2.139687330295618,"d":"2.14"},{"v":2.139687330295618,"d":"2.14"},{"v":1.0028264064999999,"d":"1.00"}]
["42025","Carbon","PA",{"v":0.26813344999999994,"d":"0.27"},{"v":2.232467745140343,"d":"2.23"},{"v":2.232467745140343,"d":"2.23"},{"v":0.9446649474999999,"d":"0.94"}]
["42027","Centre","PA",{"v":0.237085843,"d":"0.24"},{"v":2.219342616696379,"d":"2.22"},{"v":2.2193426166963794,"d":"2.22"},{"v":0.9181698165000002,"d":"0.92"}]
["42029","Chester","PA",{"v":0.23375609000000003,"d":"0.23"},{"v":1.852881370636204,"d":"1.85"},{"v":1.852881370636204,"d":"1.85"},{"v":0.6250393074999999,"d":"0.63"}]
["42031","Clarion","PA",{"v":0.284103411,"d":"0.28"},{"v":2.0230004869975486,"d":"2.02"},{"v":2.0230004869975486,"d":"2.02"},{"v":0.9005784769999998,"d":"0.90"}]
["42033","Clearfield","PA",{"v":0.26304077900000006,"d":"0.26"},{"v":2.1899212035654196,"d":"2.19"},{"v":2.1899212035654196,"d":"2.19"},{"v":0.9270977849999998,"d":"0.93"}]
["42035","Clinton","PA",{"v":0.254950929,"d":"0.25"},{"v":2.260693206368948,"d":"2.26"},{"v":2.2606932063689484,"d":"2.26"},{"v":1.0032457885000001,"d":"1.00"}]
["42037","Columbia","PA",{"v":0.267080554,"d":"0.27"},{"v":2.091931848200186,"d":"2.09"},{"v":2.0919318482001863,"d":"2.09"},{"v":0.8350854945,"d":"0.84"}]
["42039","Crawford","PA",{"v":0.28024092899999997,"d":"0.28"},{"v":2.095004727941009,"d":"2.10"},{"v":2.095004727941009,"d":"2.10"},{"v":0.8478057630000001,"d":"0.85"}]
["42041","Cumberland","PA",{"v":0.24984898599999997,"d":"0.25"},{"v":1.9620900258934733,"d":"1.96"},{"v":1.9620900258934733,"d":"1.96"},{"v":0.693573168,"d":"0.69"}]
["42043","Dauphin","PA",{"v":0.23964332299999996,"d":"0.24"},{"v":2.0256888495490775,"d":"2.03"},{"v":2.0256888495490775,"d":"2.03"},{"v":0.7170551795000001,"d":"0.72"}]
["42045","Delaware","PA",{"v":0.11371343,"d":"0.11"},{"v":0.003963268673208882,"d":"0.00"},{"v":0.003963268673208882,"d":"0.00"},{"v":0.49783811749999995,"d":"0.50"}]
["42047","Elk","PA",{"v":0.264278179,"d":"0.26"},{"v":2.0317558326143996,"d":"2.03"},{"v":2.0317558326143996,"d":"2.03"},{"v":0.968500283,"d":"0.97"}]
["42049","Erie","PA",{"v":0.239399142,"d":"0.24"},{"v":1.8891203662507914,"d":"1.89"},{"v":1.8891203662507912,"d":"1.89"},{"v":0.6983773845,"d":"0.70"}]
["42051","Fayette","PA",{"v":0.258273675,"d":"0.26"},{"v":2.0442100919895263,"d":"2.04"},{"v":2.0442100919895263,"d":"2.04"},{"v":0.8900319795000001,"d":"0.89"}]
["42053","Forest","PA",{"v":0.292056457,"d":"0.29"},{"v":2.1957793771486833,"d":"2.20"},{"v":2.1957793771486838,"d":"2.20"},{"v":1.0534747654999999,"d":"1.05"}]
["42055","Franklin","PA",{"v":0.27886464499999997,"d":"0.28"},{"v":2.0336608958344202,"d":"2.03"},{"v":2.0336608958344202,"d":"2.03"},{"v":0.7471308095000001,"d":"0.75"}]
["42057","Fulton","PA",{"v":0.302397229,"d":"0.30"},{"v":2.243078450537621,"d":"2.24"},{"v":2.243078450537621,"d":"2.24"},{"v":0.9945440695000002,"d":"0.99"}]
["42059","Greene","PA",{"v":0.284700704,"d":"0.28"},{"v":2.074738509245468,"d":"2.07"},{"v":2.074738509245468,"d":"2.07"},{"v":0.907200204,"d":"0.91"}]
["42061","Huntingdon","PA",{"v":0.27958890899999994,"d":"0.28"},{"v":2.2039746104208273,"d":"2.20"},{"v":2.2039746104208273,"d":"2.20"},{"v":0.9868543575,"d":"0.99"}]
["42063","Indiana","PA",{"v":0.269564434,"d":"0.27"},{"v":2.0096542280236016,"d":"2.01"},{"v":2.009654228023602,"d":"2.01"},{"v":0.8948277225,"d":"0.89"}]
["42065","Jefferson","PA",{"v":0.269630509,"d":"0.27"},{"v":2.033649836501574,"d":"2.03"},{"v":2.033649836501574,"d":"2.03"},{"v":0.9099681115,"d":"0.91"}]
["42067","Juniata","PA",{"v":0.290771505,"d":"0.29"},{"v":2.2243402087058666,"d":"2.22"},{"v":2.2243402087058666,"d":"2.22"},{"v":0.9406512845,"d":"0.94"}]
["42069","Lackawanna","PA",{"v":0.22037261500000002,"d":"0.22"},{"v":1.9070063657862681,"d":"1.91"},{"v":1.9070063657862686,"d":"1.91"},{"v":0.8041896245000001,"d":"0.80"}]
["42071","Lancaster","PA",{"v":0.257569238,"d":"0.26"},{"v":1.8927377108201524,"d":"1.89"},{"v":1.8927377108201524,"d":"1.89"},{"v":0.608491821,"d":"0.61"}]
["42073","Lawrence","PA",{"v":0.260273949,"d":"0.26"},{"v":1.9560665651022466,"d":"1.96"},{"v":1.9560665651022466,"d":"1.96"},{"v":0.7527660584999999,"d":"0.75"}]
["42075","Lebanon","PA",{"v":0.26844893099999995,"d":"0.27"},{"v":1.967039271071918,"d":"1.97"},{"v":1.967039271071918,"d":"1.97"},{"v":0.6918428259999999,"d":"0.69"}]
["42077","Lehigh","PA",{"v":0.21156594000000004,"d":"0.21"},{"v":1.5147673982112815,"d":"1.51"},{"v":1.5147673982112815,"d":"1.51"},{"v":0.6106994390000001,"d":"0.61"}]
["42079","Luzerne","PA",{"v":0.234049271,"d":"0.23"},{"v":2.1013933496987076,"d":"2.10"},{"v":2.1013933496987076,"d":"2.10"},{"v":0.8562137019999999,"d":"0.86"}]
["42081","Lycoming","PA",{"v":0.25349873599999995,"d":"0.25"},{"v":2.076133151141828,"d":"2.08"},{"v":2.076133151141828,"d":"2.08"},{"v":0.9115230355,"d":"0.91"}]
["42083","McKean","PA",{"v":0.27061038100000007,"d":"0.27"},{"v":2.003402902460441,"d":"2.00"},{"v":2.003402902460441,"d":"2.00"},{"v":0.9555032655000001,"d":"0.96"}]
["42085","Mercer","PA",{"v":0.262888603,"d":"0.26"},{"v":2.047645975448977,"d":"2.05"},{"v":2.0476459754489773,"d":"2.05"},{"v":0.7868163130000001,"d":"0.79"}]
["42087","Mifflin","PA",{"v":0.265375097,"d":"0.27"},{"v":2.170673587542465,"d":"2.17"},{"v":2.170673587542466,"d":"2.17"},{"v":0.9145721709999998,"d":"0.91"}]
["42089","Monroe","PA",{"v":0.240310175,"d":"0.24"},{"v":2.2647317440471832,"d":"2.26"},{"v":2.2647317440471832,"d":"2.26"},{"v":0.938992317,"d":"0.94"}]
["42091","Montgomery","PA",{"v":0.16707342299999997,"d":"0.17"},{"v":0.35708894574561906,"d":"0.36"},{"v":0.35708894574561906,"d":"0.36"},{"v":0.550982422,"d":"0.55"}]
["42093","Montour","PA",{"v":0.293564959,"d":"0.29"},{"v":2.0972502232128156,"d":"2.10"},{"v":2.097250223212815,"d":"2.10"},{"v":0.7565515755,"d":"0.76"}]
["42095","Northampton","PA",{"v":0.22112911800000004,"d":"0.22"},{"v":1.8008760662614671,"d":"1.80"},{"v":1.8008760662614673,"d":"1.80"},{"v":0.656551739,"d":"0.66"}]
["42097","Northumberland","PA",{"v":0.282625149,"d":"0.28"},{"v":2.1533431465511748,"d":"2.15"},{"v":2.1533431465511748,"d":"2.15"},{"v":0.77486577,"d":"0.77"}]
["42099","Perry","PA",{"v":0.298662209,"d":"0.30"},{"v":2.223074506620792,"d":"2.22"},{"v":2.223074506620792,"d":"2.22"},{"v":0.9364336125000001,"d":"0.94"}]
["42101","Philadelphia","PA",{"v":0.009548053,"d":"0.01"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.33043868150000005,"d":"0.33"}]
["42103","Pike","PA",{"v":0.267680298,"d":"0.27"},{"v":2.284048258971714,"d":"2.28"},{"v":2.284048258971714,"d":"2.28"},{"v":1.0302195280000002,"d":"1.03"}]
["42105","Potter","PA",{"v":0.299424728,"d":"0.30"},{"v":2.108015084831224,"d":"2.11"},{"v":2.108015084831224,"d":"2.11"},{"v":1.0014110995,"d":"1.00"}]
["42107","Schuylkill","PA",{"v":0.282157726,"d":"0.28"},{"v":2.2735019594718118,"d":"2.27"},{"v":2.2735019594718118,"d":"2.27"},{"v":0.890236838,"d":"0.89"}]
["42109","Snyder","PA",{"v":0.287501073,"d":"0.29"},{"v":2.14447614608638,"d":"2.14"},{"v":2.1444761460863795,"d":"2.14"},{"v":0.8611928350000001,"d":"0.86"}]
["42111","Somerset","PA",{"v":0.288461964,"d":"0.29"},{"v":2.1568440283148145,"d":"2.16"},{"v":2.156844028314815,"d":"2.16"},{"v":0.9177576914999999,"d":"0.92"}]
["42113","Sullivan","PA",{"v":0.296540708,"d":"0.30"},{"v":2.3654713340788787,"d":"2.37"},{"v":2.3654713340788787,"d":"2.37"},{"v":1.0403401584999998,"d":"1.04"}]
["42115","Susquehanna","PA",{"v":0.291363714,"d":"0.29"},{"v":2.285927936979823,"d":"2.29"},{"v":2.285927936979823,"d":"2.29"},{"v":0.931786621,"d":"0.93"}]
["42117","Tioga","PA",{"v":0.296230134,"d":"0.30"},{"v":2.1023127769613583,"d":"2.10"},{"v":2.102312776961358,"d":"2.10"},{"v":0.9557606585,"d":"0.96"}]
["42119","Union","PA",{"v":0.266087493,"d":"0.27"},{"v":2.152293854110021,"d":"2.15"},{"v":2.152293854110021,"d":"2.15"},{"v":0.8587123305,"d":"0.86"}]
["42121","Venango","PA",{"v":0.26063798199999993,"d":"0.26"},{"v":2.0422606356260924,"d":"2.04"},{"v":2.0422606356260924,"d":"2.04"},{"v":0.9276891919999999,"d":"0.93"}]
["42123","Warren","PA",{"v":0.2617924549999999,"d":"0.26"},{"v":2.050747088239788,"d":"2.05"},{"v":2.0507470882397882,"d":"2.05"},{"v":0.9533390275000001,"d":"0.95"}]
["42125","Washington","PA",{"v":0.255575326,"d":"0.26"},{"v":1.9476421520001772,"d":"1.95"},{"v":1.9476421520001772,"d":"1.95"},{"v":0.7606388845000001,"d":"0.76"}]
["42127","Wayne","PA",{"v":0.289991587,"d":"0.29"},{"v":2.2445201868227884,"d":"2.24"},{"v":2.244520186822788,"d":"2.24"},{"v":0.9627621994999999,"d":"0.96"}]
["42129","Westmoreland","PA",{"v":0.23350268099999996,"d":"0.23"},{"v":1.9208495493833446,"d":"1.92"},{"v":1.9208495493833442,"d":"1.92"},{"v":0.811785138,"d":"0.81"}]
["42131","Wyoming","PA",{"v":0.287385544,"d":"0.29"},{"v":2.276430255444354,"d":"2.28"},{"v":2.276430255444354,"d":"2.28"},{"v":0.9577577259999998,"d":"0.96"}]
["42133","York","PA",{"v":0.258052464,"d":"0.26"},{"v":1.9004291822548762,"d":"1.90"},{"v":1.9004291822548764,"d":"1.90"},{"v":0.6606636975000001,"d":"0.66"}]
["44001","Bristol","RI",{"v":0.140845817,"d":"0.14"},{"v":0.07911133430767722,"d":"0.08"},{"v":0.07911133430767721,"d":"0.08"},{"v":0.535945135,"d":"0.54"}]
["44003","Kent","RI",{"v":0.180298836,"d":"0.18"},{"v":1.3893569391479779,"d":"1.39"},{"v":1.3893569391479779,"d":"1.39"},{"v":0.7340686359999999,"d":"0.73"}]
["44005","Newport","RI",{"v":0.221850646,"d":"0.22"},{"v":1.589762830013043,"d":"1.59"},{"v":1.589762830013043,"d":"1.59"},{"v":0.5772089664999999,"d":"0.58"}]
["44007","Providence","RI",{"v":0.15492958,"d":"0.15"},{"v":0.5308305694213221,"d":"0.53"},{"v":0.530830569421322,"d":"0.53"},{"v":0.7070110660000001,"d":"0.71"}]
["44009","Washington","RI",{"v":0.255529383,"d":"0.26"},{"v":1.9571636705144337,"d":"1.96"},{"v":1.9571636705144337,"d":"1.96"},{"v":0.6999266035000001,"d":"0.70"}]
["45001","Abbeville","SC",{"v":0.139987702,"d":"0.14"},{"v":0.8072535909204261,"d":"0.81"},{"v":0.8072535909204259,"d":"0.81"},{"v":0.37383497000000004,"d":"0.37"}]
["45003","Aiken","SC",{"v":0.12319528299999999,"d":"0.12"},{"v":0.7815155306549957,"d":"0.78"},{"v":0.7815155306549957,"d":"0.78"},{"v":0.33610562200000005,"d":"0.34"}]
["45005","Allendale","SC",{"v":0.13515924099999999,"d":"0.14"},{"v":0.7829016844684236,"d":"0.78"},{"v":0.7829016844684235,"d":"0.78"},{"v":0.36609651949999994,"d":"0.37"}]
["45007","Anderson","SC",{"v":0.11947991100000001,"d":"0.12"},{"v":0.7866740279464978,"d":"0.79"},{"v":0.7866740279464978,"d":"0.79"},{"v":0.3181025559999999,"d":"0.32"}]
["45009","Bamberg","SC",{"v":0.132824318,"d":"0.13"},{"v":0.8005640159733323,"d":"0.80"},{"v":0.8005640159733322,"d":"0.80"},{"v":0.3632839585,"d":"0.36"}]
["45011","Barnwell","SC",{"v":0.138767965,"d":"0.14"},{"v":0.8063819428792625,"d":"0.81"},{"v":0.8063819428792626,"d":"0.81"},{"v":0.3714590315,"d":"0.37"}]
["45013","Beaufort","SC",{"v":0.123111206,"d":"0.12"},{"v":0.7621598670079069,"d":"0.76"},{"v":0.7621598670079069,"d":"0.76"},{"v":0.25464836550000003,"d":"0.25"}]
["45015","Berkeley","SC",{"v":0.11821527700000001,"d":"0.12"},{"v":0.7850317831812035,"d":"0.79"},{"v":0.7850317831812035,"d":"0.79"},{"v":0.3464176245000001,"d":"0.35"}]
["45017","Calhoun","SC",{"v":0.149917091,"d":"0.15"},{"v":0.8257587899486374,"d":"0.83"},{"v":0.8257587899486374,"d":"0.83"},{"v":0.37465196250000005,"d":"0.37"}]
["45019","Charleston","SC",{"v":0.113693726,"d":"0.11"},{"v":0.7346418323125588,"d":"0.73"},{"v":0.7346418323125588,"d":"0.73"},{"v":0.25966703899999993,"d":"0.26"}]
["45021","Cherokee","SC",{"v":0.127053902,"d":"0.13"},{"v":0.8281973637507986,"d":"0.83"},{"v":0.8281973637507987,"d":"0.83"},{"v":0.366950643,"d":"0.37"}]
["45023","Chester","SC",{"v":0.132738111,"d":"0.13"},{"v":0.7789305916016094,"d":"0.78"},{"v":0.7789305916016096,"d":"0.78"},{"v":0.399671517,"d":"0.40"}]
["45025","Chesterfield","SC",{"v":0.13813232,"d":"0.14"},{"v":0.8144116989335118,"d":"0.81"},{"v":0.814411698933512,"d":"0.81"},{"v":0.3610558805,"d":"0.36"}]
["45027","Clarendon","SC",{"v":0.143778512,"d":"0.14"},{"v":0.8374063817284957,"d":"0.84"},{"v":0.8374063817284958,"d":"0.84"},{"v":0.351900074,"d":"0.35"}]
["45029","Colleton","SC",{"v":0.13873212299999998,"d":"0.14"},{"v":0.8131876674376255,"d":"0.81"},{"v":0.8131876674376255,"d":"0.81"},{"v":0.36924136300000004,"d":"0.37"}]
["45031","Darlington","SC",{"v":0.132933803,"d":"0.13"},{"v":0.8052942414654671,"d":"0.81"},{"v":0.8052942414654671,"d":"0.81"},{"v":0.33024409849999997,"d":"0.33"}]
["45033","Dillon","SC",{"v":0.137192769,"d":"0.14"},{"v":0.8226516326118466,"d":"0.82"},{"v":0.8226516326118466,"d":"0.82"},{"v":0.35160759100000005,"d":"0.35"}]
["45035","Dorchester","SC",{"v":0.11098513899999998,"d":"0.11"},{"v":0.7694362491560538,"d":"0.77"},{"v":0.7694362491560538,"d":"0.77"},{"v":0.3487536025,"d":"0.35"}]
["45037","Edgefield","SC",{"v":0.139014638,"d":"0.14"},{"v":0.8206964343698071,"d":"0.82"},{"v":0.8206964343698071,"d":"0.82"},{"v":0.39196338,"d":"0.39"}]
["45039","Fairfield","SC",{"v":0.133041305,"d":"0.13"},{"v":0.827144240881884,"d":"0.83"},{"v":0.827144240881884,"d":"0.83"},{"v":0.4096201285,"d":"0.41"}]
["45041","Florence","SC",{"v":0.120981383,"d":"0.12"},{"v":0.7931339110126965,"d":"0.79"},{"v":0.7931339110126965,"d":"0.79"},{"v":0.340005689,"d":"0.34"}]
["45043","Georgetown","SC",{"v":0.13111618999999997,"d":"0.13"},{"v":0.8113780558669741,"d":"0.81"},{"v":0.8113780558669741,"d":"0.81"},{"v":0.3226976255,"d":"0.32"}]
["45045","Greenville","SC",{"v":0.09655214300000002,"d":"0.10"},{"v":0.7338413496322433,"d":"0.73"},{"v":0.7338413496322433,"d":"0.73"},{"v":0.315358805,"d":"0.32"}]
["45047","Greenwood","SC",{"v":0.12180817300000002,"d":"0.12"},{"v":0.7588529454028811,"d":"0.76"},{"v":0.7588529454028811,"d":"0.76"},{"v":0.36257688499999996,"d":"0.36"}]
["45049","Hampton","SC",{"v":0.137008737,"d":"0.14"},{"v":0.8166481791542469,"d":"0.82"},{"v":0.8166481791542469,"d":"0.82"},{"v":0.38204537,"d":"0.38"}]
["45051","Horry","SC",{"v":0.110185023,"d":"0.11"},{"v":0.8034928892960371,"d":"0.80"},{"v":0.8034928892960372,"d":"0.80"},{"v":0.307492614,"d":"0.31"}]
["45053","Jasper","SC",{"v":0.135765549,"d":"0.14"},{"v":0.811032911540475,"d":"0.81"},{"v":0.811032911540475,"d":"0.81"},{"v":0.3662986664999999,"d":"0.37"}]
["45055","Kershaw","SC",{"v":0.129002099,"d":"0.13"},{"v":0.8224652065869248,"d":"0.82"},{"v":0.8224652065869247,"d":"0.82"},{"v":0.364047942,"d":"0.36"}]
["45057","Lancaster","SC",{"v":0.12560720799999997,"d":"0.13"},{"v":0.758687540072183,"d":"0.76"},{"v":0.7586875400721829,"d":"0.76"},{"v":0.3720497059999999,"d":"0.37"}]
["45059","Laurens","SC",{"v":0.128766609,"d":"0.13"},{"v":0.8124810860323182,"d":"0.81"},{"v":0.812481086032318,"d":"0.81"},{"v":0.3788426605,"d":"0.38"}]
["45061","Lee","SC",{"v":0.144068571,"d":"0.14"},{"v":0.8234307047376668,"d":"0.82"},{"v":0.8234307047376668,"d":"0.82"},{"v":0.34522132050000004,"d":"0.35"}]
["45063","Lexington","SC",{"v":0.11238015400000001,"d":"0.11"},{"v":0.764537604770936,"d":"0.76"},{"v":0.7645376047709361,"d":"0.76"},{"v":0.30116036500000004,"d":"0.30"}]
["45065","McCormick","SC",{"v":0.147128205,"d":"0.15"},{"v":0.8439624622230651,"d":"0.84"},{"v":0.843962462223065,"d":"0.84"},{"v":0.4028589469999999,"d":"0.40"}]
["45067","Marion","SC",{"v":0.13204920800000003,"d":"0.13"},{"v":0.809495106119623,"d":"0.81"},{"v":0.8094951061196232,"d":"0.81"},{"v":0.37266817850000006,"d":"0.37"}]
["45069","Marlboro","SC",{"v":0.134079292,"d":"0.13"},{"v":0.7998567037683773,"d":"0.80"},{"v":0.7998567037683773,"d":"0.80"},{"v":0.3539116505,"d":"0.35"}]
["45071","Newberry","SC",{"v":0.133286883,"d":"0.13"},{"v":0.7975396028782565,"d":"0.80"},{"v":0.7975396028782565,"d":"0.80"},{"v":0.38158536500000007,"d":"0.38"}]
["45073","Oconee","SC",{"v":0.12860525900000003,"d":"0.13"},{"v":0.8179705978197586,"d":"0.82"},{"v":0.8179705978197583,"d":"0.82"},{"v":0.38148766000000006,"d":"0.38"}]
["45075","Orangeburg","SC",{"v":0.135974574,"d":"0.14"},{"v":0.8079318682270916,"d":"0.81"},{"v":0.8079318682270916,"d":"0.81"},{"v":0.35253657499999996,"d":"0.35"}]
["45077","Pickens","SC",{"v":0.113384433,"d":"0.11"},{"v":0.7884327299116517,"d":"0.79"},{"v":0.7884327299116517,"d":"0.79"},{"v":0.354966884,"d":"0.35"}]
["45079","Richland","SC",{"v":0.09774187900000002,"d":"0.10"},{"v":0.7253915004724751,"d":"0.73"},{"v":0.7253915004724752,"d":"0.73"},{"v":0.31501126549999997,"d":"0.32"}]
["45081","Saluda","SC",{"v":0.140538586,"d":"0.14"},{"v":0.830361748028576,"d":"0.83"},{"v":0.8303617480285761,"d":"0.83"},{"v":0.3756491855000001,"d":"0.38"}]
["45083","Spartanburg","SC",{"v":0.10991045399999999,"d":"0.11"},{"v":0.7797497247286056,"d":"0.78"},{"v":0.7797497247286056,"d":"0.78"},{"v":0.32722526150000003,"d":"0.33"}]
["45085","Sumter","SC",{"v":0.12116754200000003,"d":"0.12"},{"v":0.7996015573306501,"d":"0.80"},{"v":0.7996015573306501,"d":"0.80"},{"v":0.33072551450000004,"d":"0.33"}]
["45087","Union","SC",{"v":0.12851242399999996,"d":"0.13"},{"v":0.8059499353717542,"d":"0.81"},{"v":0.805949935371754,"d":"0.81"},{"v":0.4040356955,"d":"0.40"}]
["45089","Williamsburg","SC",{"v":0.138766862,"d":"0.14"},{"v":0.8385536844798059,"d":"0.84"},{"v":0.8385536844798059,"d":"0.84"},{"v":0.38286616349999997,"d":"0.38"}]
["45091","York","SC",{"v":0.109630662,"d":"0.11"},{"v":0.7640991296108991,"d":"0.76"},{"v":0.7640991296108991,"d":"0.76"},{"v":0.33397133900000003,"d":"0.33"}]
["46003","Aurora","SD",{"v":0.24601584099999999,"d":"0.25"},{"v":1.5880008274560782,"d":"1.59"},{"v":1.588000827456078,"d":"1.59"},{"v":0.5247814745,"d":"0.52"}]
["46005","Beadle","SD",{"v":0.19636334,"d":"0.20"},{"v":1.5846586231427107,"d":"1.58"},{"v":1.5846586231427107,"d":"1.58"},{"v":0.45901796600000005,"d":"0.46"}]
["46007","Bennett","SD",{"v":0.247455106,"d":"0.25"},{"v":1.5744371355468072,"d":"1.57"},{"v":1.5744371355468068,"d":"1.57"},{"v":0.5225735539999999,"d":"0.52"}]
["46009","Bon Homme","SD",{"v":0.240365543,"d":"0.24"},{"v":1.5938801326977612,"d":"1.59"},{"v":1.5938801326977612,"d":"1.59"},{"v":0.5255019145000001,"d":"0.53"}]
["46011","Brookings","SD",{"v":0.192215584,"d":"0.19"},{"v":1.5939339092838014,"d":"1.59"},{"v":1.5939339092838014,"d":"1.59"},{"v":0.4648250060000001,"d":"0.46"}]
["46013","Brown","SD",{"v":0.19214834300000003,"d":"0.19"},{"v":1.5961741254184338,"d":"1.60"},{"v":1.5961741254184338,"d":"1.60"},{"v":0.4669082574999999,"d":"0.47"}]
["46015","Brule","SD",{"v":0.24119806100000002,"d":"0.24"},{"v":1.599365306372926,"d":"1.60"},{"v":1.5993653063729263,"d":"1.60"},{"v":0.5289162125000001,"d":"0.53"}]
["46017","Buffalo","SD",{"v":0.243260921,"d":"0.24"},{"v":1.6019419550196468,"d":"1.60"},{"v":1.6019419550196468,"d":"1.60"},{"v":0.5281319159999999,"d":"0.53"}]
["46019","Butte","SD",{"v":0.208197544,"d":"0.21"},{"v":1.5896857068267798,"d":"1.59"},{"v":1.5896857068267796,"d":"1.59"},{"v":0.4912419695000001,"d":"0.49"}]
["46021","Campbell","SD",{"v":0.241065564,"d":"0.24"},{"v":1.6549228987248228,"d":"1.65"},{"v":1.6549228987248226,"d":"1.65"},{"v":0.538162516,"d":"0.54"}]
["46023","Charles Mix","SD",{"v":0.242085717,"d":"0.24"},{"v":1.5900832233727311,"d":"1.59"},{"v":1.5900832233727311,"d":"1.59"},{"v":0.5280226145000001,"d":"0.53"}]
["46025","Clark","SD",{"v":0.24258989,"d":"0.24"},{"v":1.6100307352090013,"d":"1.61"},{"v":1.6100307352090009,"d":"1.61"},{"v":0.533489717,"d":"0.53"}]
["46027","Clay","SD",{"v":0.194191868,"d":"0.19"},{"v":1.5258466543496227,"d":"1.53"},{"v":1.525846654349623,"d":"1.53"},{"v":0.45846739999999997,"d":"0.46"}]
["46029","Codington","SD",{"v":0.19253850599999997,"d":"0.19"},{"v":1.5658680126877624,"d":"1.57"},{"v":1.5658680126877624,"d":"1.57"},{"v":0.45222887249999993,"d":"0.45"}]
["46031","Corson","SD",{"v":0.242292886,"d":"0.24"},{"v":1.6503268134294142,"d":"1.65"},{"v":1.6503268134294142,"d":"1.65"},{"v":0.5418400764999999,"d":"0.54"}]
["46033","Custer","SD",{"v":0.233398057,"d":"0.23"},{"v":1.645660330430524,"d":"1.65"},{"v":1.645660330430524,"d":"1.65"},{"v":0.562021246,"d":"0.56"}]
["46035","Davison","SD",{"v":0.19233769899999997,"d":"0.19"},{"v":1.500396990664948,"d":"1.50"},{"v":1.500396990664948,"d":"1.50"},{"v":0.4454439320000001,"d":"0.45"}]
["46037","Day","SD",{"v":0.239461142,"d":"0.24"},{"v":1.652251689746606,"d":"1.65"},{"v":1.652251689746606,"d":"1.65"},{"v":0.539919189,"d":"0.54"}]
["46039","Deuel","SD",{"v":0.23875467200000003,"d":"0.24"},{"v":1.6251998391652183,"d":"1.63"},{"v":1.625199839165218,"d":"1.63"},{"v":0.5327674179999998,"d":"0.53"}]
["46041","Dewey","SD",{"v":0.21390091300000003,"d":"0.21"},{"v":1.6237557651798677,"d":"1.62"},{"v":1.6237557651798682,"d":"1.62"},{"v":0.5153452855000001,"d":"0.52"}]
["46043","Douglas","SD",{"v":0.24206861700000004,"d":"0.24"},{"v":1.596675678913583,"d":"1.60"},{"v":1.596675678913583,"d":"1.60"},{"v":0.5213940545,"d":"0.52"}]
["46045","Edmunds","SD",{"v":0.23981342099999997,"d":"0.24"},{"v":1.6344631919619867,"d":"1.63"},{"v":1.634463191961987,"d":"1.63"},{"v":0.537010657,"d":"0.54"}]
["46047","Fall River","SD",{"v":0.20969017999999998,"d":"0.21"},{"v":1.6060355640553365,"d":"1.61"},{"v":1.6060355640553363,"d":"1.61"},{"v":0.49031683000000004,"d":"0.49"}]
["46049","Faulk","SD",{"v":0.240227233,"d":"0.24"},{"v":1.640702088896714,"d":"1.64"},{"v":1.640702088896714,"d":"1.64"},{"v":0.538591113,"d":"0.54"}]
["46051","Grant","SD",{"v":0.210348314,"d":"0.21"},{"v":1.6222848089549162,"d":"1.62"},{"v":1.6222848089549158,"d":"1.62"},{"v":0.49651905000000013,"d":"0.50"}]
["46053","Gregory","SD",{"v":0.24207672399999997,"d":"0.24"},{"v":1.5840631707254156,"d":"1.58"},{"v":1.5840631707254156,"d":"1.58"},{"v":0.5282926560000001,"d":"0.53"}]
["46055","Haakon","SD",{"v":0.24268182900000002,"d":"0.24"},{"v":1.577642648819246,"d":"1.58"},{"v":1.577642648819246,"d":"1.58"},{"v":0.5223440045000001,"d":"0.52"}]
["46057","Hamlin","SD",{"v":0.240089561,"d":"0.24"},{"v":1.6159948260438146,"d":"1.62"},{"v":1.6159948260438144,"d":"1.62"},{"v":0.5325536435,"d":"0.53"}]
["46059","Hand","SD",{"v":0.23965602599999997,"d":"0.24"},{"v":1.6357711085891204,"d":"1.64"},{"v":1.6357711085891202,"d":"1.64"},{"v":0.533999003,"d":"0.53"}]
["46061","Hanson","SD",{"v":0.24640086100000003,"d":"0.25"},{"v":1.5856605330749642,"d":"1.59"},{"v":1.5856605330749642,"d":"1.59"},{"v":0.5216439765,"d":"0.52"}]
["46063","Harding","SD",{"v":0.238537994,"d":"0.24"},{"v":1.64961195766036,"d":"1.65"},{"v":1.64961195766036,"d":"1.65"},{"v":0.5409378995,"d":"0.54"}]
["46065","Hughes","SD",{"v":0.193916874,"d":"0.19"},{"v":1.550852210655589,"d":"1.55"},{"v":1.550852210655589,"d":"1.55"},{"v":0.449060193,"d":"0.45"}]
["46067","Hutchinson","SD",{"v":0.244868795,"d":"0.24"},{"v":1.5721248486255797,"d":"1.57"},{"v":1.5721248486255797,"d":"1.57"},{"v":0.5203517885000001,"d":"0.52"}]
["46069","Hyde","SD",{"v":0.24363550800000003,"d":"0.24"},{"v":1.603253312228996,"d":"1.60"},{"v":1.603253312228996,"d":"1.60"},{"v":0.5247412115000001,"d":"0.52"}]
["46071","Jackson","SD",{"v":0.243508659,"d":"0.24"},{"v":1.5787668903061916,"d":"1.58"},{"v":1.5787668903061918,"d":"1.58"},{"v":0.526416083,"d":"0.53"}]
["46073","Jerauld","SD",{"v":0.23781809799999998,"d":"0.24"},{"v":1.640823857877721,"d":"1.64"},{"v":1.6408238578777208,"d":"1.64"},{"v":0.5341071935,"d":"0.53"}]
["46075","Jones","SD",{"v":0.242019591,"d":"0.24"},{"v":1.6006293069991837,"d":"1.60"},{"v":1.6006293069991837,"d":"1.60"},{"v":0.5318366440000001,"d":"0.53"}]
["46077","Kingsbury","SD",{"v":0.24192377699999998,"d":"0.24"},{"v":1.6110865924299924,"d":"1.61"},{"v":1.6110865924299922,"d":"1.61"},{"v":0.5330084734999999,"d":"0.53"}]
["46079","Lake","SD",{"v":0.206458835,"d":"0.21"},{"v":1.5968712915029275,"d":"1.60"},{"v":1.5968712915029275,"d":"1.60"},{"v":0.481733008,"d":"0.48"}]
["46081","Lawrence","SD",{"v":0.187027613,"d":"0.19"},{"v":1.6018769710845768,"d":"1.60"},{"v":1.601876971084577,"d":"1.60"},{"v":0.553489501,"d":"0.55"}]
["46083","Lincoln","SD",{"v":0.200412362,"d":"0.20"},{"v":1.5251014116332244,"d":"1.53"},{"v":1.5251014116332244,"d":"1.53"},{"v":0.45101663750000004,"d":"0.45"}]
["46085","Lyman","SD",{"v":0.24146083,"d":"0.24"},{"v":1.6031817947287677,"d":"1.60"},{"v":1.6031817947287679,"d":"1.60"},{"v":0.5286998350000001,"d":"0.53"}]
["46087","McCook","SD",{"v":0.247197405,"d":"0.25"},{"v":1.5602844088697392,"d":"1.56"},{"v":1.5602844088697392,"d":"1.56"},{"v":0.5226044819999999,"d":"0.52"}]
["46089","McPherson","SD",{"v":0.24240698000000002,"d":"0.24"},{"v":1.6437517774159893,"d":"1.64"},{"v":1.643751777415989,"d":"1.64"},{"v":0.5363090085,"d":"0.54"}]
["46091","Marshall","SD",{"v":0.23684462399999998,"d":"0.24"},{"v":1.656674296425233,"d":"1.66"},{"v":1.656674296425233,"d":"1.66"},{"v":0.5438495455000001,"d":"0.54"}]
["46093","Meade","SD",{"v":0.21038871699999998,"d":"0.21"},{"v":1.5973116152580258,"d":"1.60"},{"v":1.5973116152580258,"d":"1.60"},{"v":0.48007228399999996,"d":"0.48"}]
["46095","Mellette","SD",{"v":0.24765424,"d":"0.25"},{"v":1.5765010306334684,"d":"1.58"},{"v":1.5765010306334684,"d":"1.58"},{"v":0.5240781470000001,"d":"0.52"}]
["46097","Miner","SD",{"v":0.242376022,"d":"0.24"},{"v":1.6007280035944789,"d":"1.60"},{"v":1.6007280035944789,"d":"1.60"},{"v":0.5350460170000001,"d":"0.54"}]
["46099","Minnehaha","SD",{"v":0.17443647500000004,"d":"0.17"},{"v":1.4821520473879146,"d":"1.48"},{"v":1.4821520473879146,"d":"1.48"},{"v":0.4233395149999999,"d":"0.42"}]
["46101","Moody","SD",{"v":0.240573377,"d":"0.24"},{"v":1.6245693070665843,"d":"1.62"},{"v":1.6245693070665843,"d":"1.62"},{"v":0.5337147309999999,"d":"0.53"}]
["46102","Oglala Lakota","SD",{"v":0.2271359698615384,"d":"0.23"},{"v":1.6,"d":"1.60"},{"v":1.6,"d":"1.60"},{"v":0.5122886106692307,"d":"0.51"}]
["46103","Pennington","SD",{"v":0.19065981500000004,"d":"0.19"},{"v":1.503492686386943,"d":"1.50"},{"v":1.503492686386943,"d":"1.50"},{"v":0.4615304420000001,"d":"0.46"}]
["46105","Perkins","SD",{"v":0.24094269,"d":"0.24"},{"v":1.635832102147915,"d":"1.64"},{"v":1.6358321021479152,"d":"1.64"},{"v":0.5344094675000001,"d":"0.53"}]
["46107","Potter","SD",{"v":0.23618588599999998,"d":"0.24"},{"v":1.6540420497260138,"d":"1.65"},{"v":1.6540420497260138,"d":"1.65"},{"v":0.54492463,"d":"0.54"}]
["46109","Roberts","SD",{"v":0.23646019300000004,"d":"0.24"},{"v":1.6585421053637488,"d":"1.66"},{"v":1.6585421053637486,"d":"1.66"},{"v":0.5421886860000001,"d":"0.54"}]
["46111","Sanborn","SD",{"v":0.24123743,"d":"0.24"},{"v":1.6335196431590413,"d":"1.63"},{"v":1.633519643159041,"d":"1.63"},{"v":0.5376465490000001,"d":"0.54"}]
["46115","Spink","SD",{"v":0.239462412,"d":"0.24"},{"v":1.608951712324287,"d":"1.61"},{"v":1.608951712324287,"d":"1.61"},{"v":0.5354917464999999,"d":"0.54"}]
["46117","Stanley","SD",{"v":0.20404406,"d":"0.20"},{"v":1.580404443238669,"d":"1.58"},{"v":1.580404443238669,"d":"1.58"},{"v":0.4761725455000001,"d":"0.48"}]
["46119","Sully","SD",{"v":0.24531151200000004,"d":"0.25"},{"v":1.598315609908934,"d":"1.60"},{"v":1.5983156099089337,"d":"1.60"},{"v":0.5254063135000001,"d":"0.53"}]
["46121","Todd","SD",{"v":0.23907301999999997,"d":"0.24"},{"v":1.5655655365371737,"d":"1.57"},{"v":1.5655655365371737,"d":"1.57"},{"v":0.5266442370000001,"d":"0.53"}]
["46123","Tripp","SD",{"v":0.213946135,"d":"0.21"},{"v":1.56407203305529,"d":"1.56"},{"v":1.56407203305529,"d":"1.56"},{"v":0.47265179850000005,"d":"0.47"}]
["46125","Turner","SD",{"v":0.243780317,"d":"0.24"},{"v":1.5718593995987507,"d":"1.57"},{"v":1.5718593995987509,"d":"1.57"},{"v":0.5216411469999999,"d":"0.52"}]
["46127","Union","SD",{"v":0.214148922,"d":"0.21"},{"v":1.5458960249867122,"d":"1.55"},{"v":1.545896024986712,"d":"1.55"},{"v":0.4952611465,"d":"0.50"}]
["46129","Walworth","SD",{"v":0.200724508,"d":"0.20"},{"v":1.6162572991827706,"d":"1.62"},{"v":1.6162572991827708,"d":"1.62"},{"v":0.47838282549999983,"d":"0.48"}]
["46135","Yankton","SD",{"v":0.198907131,"d":"0.20"},{"v":1.5305536240537825,"d":"1.53"},{"v":1.5305536240537827,"d":"1.53"},{"v":0.46356638899999997,"d":"0.46"}]
["46137","Ziebach","SD",{"v":0.222597271,"d":"0.22"},{"v":1.6273929014465833,"d":"1.63"},{"v":1.6273929014465836,"d":"1.63"},{"v":0.5261580465000001,"d":"0.53"}]
["47001","Anderson","TN",{"v":0.15176452,"d":"0.15"},{"v":1.1123041189275829,"d":"1.11"},{"v":1.1123041189275829,"d":"1.11"},{"v":0.5033665405,"d":"0.50"}]
["47003","Bedford","TN",{"v":0.184101326,"d":"0.18"},{"v":1.1280042607263363,"d":"1.13"},{"v":1.1280042607263363,"d":"1.13"},{"v":0.4288844214999999,"d":"0.43"}]
["47005","Benton","TN",{"v":0.18559122099999997,"d":"0.19"},{"v":1.1364462189603237,"d":"1.14"},{"v":1.136446218960324,"d":"1.14"},{"v":0.512451131,"d":"0.51"}]
["47007","Bledsoe","TN",{"v":0.19186620199999999,"d":"0.19"},{"v":1.1934975591338786,"d":"1.19"},{"v":1.1934975591338786,"d":"1.19"},{"v":0.552194466,"d":"0.55"}]
["47009","Blount","TN",{"v":0.15351155600000002,"d":"0.15"},{"v":1.1427448025151015,"d":"1.14"},{"v":1.1427448025151015,"d":"1.14"},{"v":0.4883758330000001,"d":"0.49"}]
["47011","Bradley","TN",{"v":0.155643381,"d":"0.16"},{"v":1.122571204376747,"d":"1.12"},{"v":1.122571204376747,"d":"1.12"},{"v":0.446005248,"d":"0.45"}]
["47013","Campbell","TN",{"v":0.163865759,"d":"0.16"},{"v":1.161150841133933,"d":"1.16"},{"v":1.161150841133933,"d":"1.16"},{"v":0.5573136725,"d":"0.56"}]
["47015","Cannon","TN",{"v":0.189517526,"d":"0.19"},{"v":1.142715459483156,"d":"1.14"},{"v":1.1427154594831557,"d":"1.14"},{"v":0.49537282699999996,"d":"0.50"}]
["47017","Carroll","TN",{"v":0.19309103500000002,"d":"0.19"},{"v":1.0976219705392931,"d":"1.10"},{"v":1.0976219705392931,"d":"1.10"},{"v":0.49227581800000003,"d":"0.49"}]
["47019","Carter","TN",{"v":0.154509164,"d":"0.15"},{"v":1.1806305507248378,"d":"1.18"},{"v":1.1806305507248376,"d":"1.18"},{"v":0.5406240975,"d":"0.54"}]
["47021","Cheatham","TN",{"v":0.18185484400000002,"d":"0.18"},{"v":1.1430288081942754,"d":"1.14"},{"v":1.1430288081942754,"d":"1.14"},{"v":0.5259929340000001,"d":"0.53"}]
["47023","Chester","TN",{"v":0.181574098,"d":"0.18"},{"v":1.086112906280178,"d":"1.09"},{"v":1.086112906280178,"d":"1.09"},{"v":0.5070688230000001,"d":"0.51"}]
["47025","Claiborne","TN",{"v":0.17823269900000002,"d":"0.18"},{"v":1.1943827936220164,"d":"1.19"},{"v":1.1943827936220166,"d":"1.19"},{"v":0.5289166145,"d":"0.53"}]
["47027","Clay","TN",{"v":0.192926134,"d":"0.19"},{"v":1.1937864755078034,"d":"1.19"},{"v":1.1937864755078034,"d":"1.19"},{"v":0.5494015610000001,"d":"0.55"}]
["47029","Cocke","TN",{"v":0.171195848,"d":"0.17"},{"v":1.1817369057441482,"d":"1.18"},{"v":1.1817369057441482,"d":"1.18"},{"v":0.5490943425,"d":"0.55"}]
["47031","Coffee","TN",{"v":0.172257846,"d":"0.17"},{"v":1.1220893030439454,"d":"1.12"},{"v":1.1220893030439456,"d":"1.12"},{"v":0.44986387949999984,"d":"0.45"}]
["47033","Crockett","TN",{"v":0.200811783,"d":"0.20"},{"v":1.095064542355178,"d":"1.10"},{"v":1.0950645423551781,"d":"1.10"},{"v":0.407597194,"d":"0.41"}]
["47035","Cumberland","TN",{"v":0.17303235299999997,"d":"0.17"},{"v":1.1330480022692981,"d":"1.13"},{"v":1.1330480022692981,"d":"1.13"},{"v":0.535897207,"d":"0.54"}]
["47037","Davidson","TN",{"v":0.10089782499999998,"d":"0.10"},{"v":0.4250717051422153,"d":"0.43"},{"v":0.4250717051422154,"d":"0.43"},{"v":0.36394799699999997,"d":"0.36"}]
["47039","Decatur","TN",{"v":0.197258506,"d":"0.20"},{"v":1.1044318842294671,"d":"1.10"},{"v":1.1044318842294671,"d":"1.10"},{"v":0.5292837340000001,"d":"0.53"}]
["47041","Dekalb","TN",{"v":0.187443892,"d":"0.19"},{"v":1.0734312997948998,"d":"1.07"},{"v":1.0734312997948998,"d":"1.07"},{"v":0.5012245835,"d":"0.50"}]
["47043","Dickson","TN",{"v":0.177289897,"d":"0.18"},{"v":1.089895812942179,"d":"1.09"},{"v":1.089895812942179,"d":"1.09"},{"v":0.4986705489999999,"d":"0.50"}]
["47045","Dyer","TN",{"v":0.186290338,"d":"0.19"},{"v":1.0689921815439138,"d":"1.07"},{"v":1.0689921815439138,"d":"1.07"},{"v":0.3902201135,"d":"0.39"}]
["47047","Fayette","TN",{"v":0.19486267099999996,"d":"0.19"},{"v":1.0825010468185954,"d":"1.08"},{"v":1.0825010468185956,"d":"1.08"},{"v":0.47336648349999993,"d":"0.47"}]
["47049","Fentress","TN",{"v":0.18828725199999996,"d":"0.19"},{"v":1.176523973139553,"d":"1.18"},{"v":1.1765239731395531,"d":"1.18"},{"v":0.596329408,"d":"0.60"}]
["47051","Franklin","TN",{"v":0.180367789,"d":"0.18"},{"v":1.1284127000535606,"d":"1.13"},{"v":1.1284127000535606,"d":"1.13"},{"v":0.5135771834999999,"d":"0.51"}]
["47053","Gibson","TN",{"v":0.187116749,"d":"0.19"},{"v":1.0718416164122266,"d":"1.07"},{"v":1.0718416164122266,"d":"1.07"},{"v":0.401176406,"d":"0.40"}]
["47055","Giles","TN",{"v":0.187803525,"d":"0.19"},{"v":1.1389668007613758,"d":"1.14"},{"v":1.138966800761376,"d":"1.14"},{"v":0.48141651550000003,"d":"0.48"}]
["47057","Grainger","TN",{"v":0.195002911,"d":"0.20"},{"v":1.2193262813981816,"d":"1.22"},{"v":1.2193262813981813,"d":"1.22"},{"v":0.5103955219999999,"d":"0.51"}]
["47059","Greene","TN",{"v":0.182711764,"d":"0.18"},{"v":1.1812769209225222,"d":"1.18"},{"v":1.1812769209225222,"d":"1.18"},{"v":0.45831694249999994,"d":"0.46"}]
["47061","Grundy","TN",{"v":0.18801645699999997,"d":"0.19"},{"v":1.2264336675227718,"d":"1.23"},{"v":1.2264336675227718,"d":"1.23"},{"v":0.5742401885000001,"d":"0.57"}]
["47063","Hamblen","TN",{"v":0.153778946,"d":"0.15"},{"v":1.0957650791892324,"d":"1.10"},{"v":1.0957650791892322,"d":"1.10"},{"v":0.385435586,"d":"0.39"}]
["47065","Hamilton","TN",{"v":0.126905594,"d":"0.13"},{"v":1.017846515505937,"d":"1.02"},{"v":1.017846515505937,"d":"1.02"},{"v":0.429005074,"d":"0.43"}]
["47067","Hancock","TN",{"v":0.193143883,"d":"0.19"},{"v":1.2172527672934141,"d":"1.22"},{"v":1.2172527672934141,"d":"1.22"},{"v":0.5586425305000001,"d":"0.56"}]
["47069","Hardeman","TN",{"v":0.184383519,"d":"0.18"},{"v":1.0995306086301697,"d":"1.10"},{"v":1.0995306086301697,"d":"1.10"},{"v":0.5348408364999999,"d":"0.53"}]
["47071","Hardin","TN",{"v":0.182413375,"d":"0.18"},{"v":1.1090144836575837,"d":"1.11"},{"v":1.1090144836575837,"d":"1.11"},{"v":0.5152954675,"d":"0.52"}]
["47073","Hawkins","TN",{"v":0.170659442,"d":"0.17"},{"v":1.1731369829790805,"d":"1.17"},{"v":1.1731369829790808,"d":"1.17"},{"v":0.4870800215,"d":"0.49"}]
["47075","Haywood","TN",{"v":0.187013651,"d":"0.19"},{"v":1.0634325447975217,"d":"1.06"},{"v":1.0634325447975217,"d":"1.06"},{"v":0.4187904595,"d":"0.42"}]
["47077","Henderson","TN",{"v":0.18976917200000004,"d":"0.19"},{"v":1.0712822446600825,"d":"1.07"},{"v":1.0712822446600825,"d":"1.07"},{"v":0.49277178650000003,"d":"0.49"}]
["47079","Henry","TN",{"v":0.18444109400000003,"d":"0.18"},{"v":1.1171947709064696,"d":"1.12"},{"v":1.1171947709064696,"d":"1.12"},{"v":0.4689468265000001,"d":"0.47"}]
["47081","Hickman","TN",{"v":0.192287452,"d":"0.19"},{"v":1.1684662604750864,"d":"1.17"},{"v":1.1684662604750864,"d":"1.17"},{"v":0.5516709365,"d":"0.55"}]
["47083","Houston","TN",{"v":0.193940686,"d":"0.19"},{"v":1.184737674387576,"d":"1.18"},{"v":1.1847376743875762,"d":"1.18"},{"v":0.5454708220000001,"d":"0.55"}]
["47085","Humphreys","TN",{"v":0.18640693499999997,"d":"0.19"},{"v":1.1050185358803462,"d":"1.11"},{"v":1.1050185358803462,"d":"1.11"},{"v":0.531668195,"d":"0.53"}]
["47087","Jackson","TN",{"v":0.190638447,"d":"0.19"},{"v":1.204242660920046,"d":"1.20"},{"v":1.2042426609200458,"d":"1.20"},{"v":0.564501512,"d":"0.56"}]
["47089","Jefferson","TN",{"v":0.17961872,"d":"0.18"},{"v":1.1625081893310703,"d":"1.16"},{"v":1.1625081893310703,"d":"1.16"},{"v":0.4344332425,"d":"0.43"}]
["47091","Johnson","TN",{"v":0.17825170899999998,"d":"0.18"},{"v":1.2122141516645522,"d":"1.21"},{"v":1.2122141516645522,"d":"1.21"},{"v":0.5856245669999999,"d":"0.59"}]
["47093","Knox","TN",{"v":0.12194900100000002,"d":"0.12"},{"v":0.9019317631989671,"d":"0.90"},{"v":0.901931763198967,"d":"0.90"},{"v":0.3895349940000001,"d":"0.39"}]
["47095","Lake","TN",{"v":0.21511155700000004,"d":"0.22"},{"v":1.0533129295875594,"d":"1.05"},{"v":1.0533129295875594,"d":"1.05"},{"v":0.4396869955,"d":"0.44"}]
["47097","Lauderdale","TN",{"v":0.187659782,"d":"0.19"},{"v":1.0490058011773669,"d":"1.05"},{"v":1.0490058011773669,"d":"1.05"},{"v":0.4259098734999999,"d":"0.43"}]
["47099","Lawrence","TN",{"v":0.187726812,"d":"0.19"},{"v":1.1165242028755804,"d":"1.12"},{"v":1.1165242028755804,"d":"1.12"},{"v":0.479294662,"d":"0.48"}]
["47101","Lewis","TN",{"v":0.18084089600000003,"d":"0.18"},{"v":1.1306354616182908,"d":"1.13"},{"v":1.1306354616182908,"d":"1.13"},{"v":0.535320674,"d":"0.54"}]
["47103","Lincoln","TN",{"v":0.190623795,"d":"0.19"},{"v":1.1205605140699275,"d":"1.12"},{"v":1.1205605140699273,"d":"1.12"},{"v":0.4586294195000001,"d":"0.46"}]
["47105","Loudon","TN",{"v":0.168930964,"d":"0.17"},{"v":1.1322575293345425,"d":"1.13"},{"v":1.1322575293345425,"d":"1.13"},{"v":0.42238786799999994,"d":"0.42"}]
["47107","McMinn","TN",{"v":0.176423848,"d":"0.18"},{"v":1.1431145485708591,"d":"1.14"},{"v":1.1431145485708591,"d":"1.14"},{"v":0.4704174945,"d":"0.47"}]
["47109","McNairy","TN",{"v":0.18763519199999998,"d":"0.19"},{"v":1.1606344304579137,"d":"1.16"},{"v":1.1606344304579137,"d":"1.16"},{"v":0.5353871600000001,"d":"0.54"}]
["47111","Macon","TN",{"v":0.185672212,"d":"0.19"},{"v":1.1619185790710365,"d":"1.16"},{"v":1.1619185790710365,"d":"1.16"},{"v":0.49837547,"d":"0.50"}]
["47113","Madison","TN",{"v":0.162404216,"d":"0.16"},{"v":1.049988997985419,"d":"1.05"},{"v":1.049988997985419,"d":"1.05"},{"v":0.43022582149999994,"d":"0.43"}]
["47115","Marion","TN",{"v":0.17541510399999996,"d":"0.18"},{"v":1.1686741575689203,"d":"1.17"},{"v":1.1686741575689203,"d":"1.17"},{"v":0.573401948,"d":"0.57"}]
["47117","Marshall","TN",{"v":0.18506070100000002,"d":"0.19"},{"v":1.136820842230982,"d":"1.14"},{"v":1.136820842230982,"d":"1.14"},{"v":0.4545555095,"d":"0.45"}]
["47119","Maury","TN",{"v":0.17069964999999998,"d":"0.17"},{"v":1.0979649074403126,"d":"1.10"},{"v":1.0979649074403124,"d":"1.10"},{"v":0.44058579800000003,"d":"0.44"}]
["47121","Meigs","TN",{"v":0.19881371800000003,"d":"0.20"},{"v":1.213207381654697,"d":"1.21"},{"v":1.2132073816546973,"d":"1.21"},{"v":0.5078042445000001,"d":"0.51"}]
["47123","Monroe","TN",{"v":0.176586218,"d":"0.18"},{"v":1.1975473406595007,"d":"1.20"},{"v":1.1975473406595007,"d":"1.20"},{"v":0.5519253885000002,"d":"0.55"}]
["47125","Montgomery","TN",{"v":0.150734509,"d":"0.15"},{"v":1.0939673259472948,"d":"1.09"},{"v":1.093967325947295,"d":"1.09"},{"v":0.4128400605,"d":"0.41"}]
["47127","Moore","TN",{"v":0.20399407100000003,"d":"0.20"},{"v":1.1684628999472606,"d":"1.17"},{"v":1.1684628999472606,"d":"1.17"},{"v":0.49339156650000016,"d":"0.49"}]
["47129","Morgan","TN",{"v":0.18378140399999998,"d":"0.18"},{"v":1.1669530308687495,"d":"1.17"},{"v":1.1669530308687492,"d":"1.17"},{"v":0.6063899334999999,"d":"0.61"}]
["47131","Obion","TN",{"v":0.196229139,"d":"0.20"},{"v":1.0882821322608252,"d":"1.09"},{"v":1.0882821322608254,"d":"1.09"},{"v":0.40948213299999986,"d":"0.41"}]
["47133","Overton","TN",{"v":0.18356554800000002,"d":"0.18"},{"v":1.1939587306088073,"d":"1.19"},{"v":1.1939587306088073,"d":"1.19"},{"v":0.5494339115000001,"d":"0.55"}]
["47135","Perry","TN",{"v":0.191270471,"d":"0.19"},{"v":1.1891944307348308,"d":"1.19"},{"v":1.189194430734831,"d":"1.19"},{"v":0.5656485485000001,"d":"0.57"}]
["47137","Pickett","TN",{"v":0.18855778900000003,"d":"0.19"},{"v":1.2249812870316656,"d":"1.22"},{"v":1.2249812870316656,"d":"1.22"},{"v":0.5674461540000001,"d":"0.57"}]
["47139","Polk","TN",{"v":0.186572002,"d":"0.19"},{"v":1.2229341421173487,"d":"1.22"},{"v":1.2229341421173487,"d":"1.22"},{"v":0.6078967239999999,"d":"0.61"}]
["47141","Putnam","TN",{"v":0.15593107100000003,"d":"0.16"},{"v":1.1261196897179702,"d":"1.13"},{"v":1.12611968971797,"d":"1.13"},{"v":0.49295759149999996,"d":"0.49"}]
["47143","Rhea","TN",{"v":0.179851941,"d":"0.18"},{"v":1.1264688523219493,"d":"1.13"},{"v":1.1264688523219495,"d":"1.13"},{"v":0.5077526509999999,"d":"0.51"}]
["47145","Roane","TN",{"v":0.168536988,"d":"0.17"},{"v":1.1315047720926874,"d":"1.13"},{"v":1.1315047720926872,"d":"1.13"},{"v":0.486039674,"d":"0.49"}]
["47147","Robertson","TN",{"v":0.18294209799999997,"d":"0.18"},{"v":1.0977507613028503,"d":"1.10"},{"v":1.0977507613028505,"d":"1.10"},{"v":0.41468288900000005,"d":"0.41"}]
["47149","Rutherford","TN",{"v":0.146854561,"d":"0.15"},{"v":1.0812822019727222,"d":"1.08"},{"v":1.0812822019727222,"d":"1.08"},{"v":0.37956609950000003,"d":"0.38"}]
["47151","Scott","TN",{"v":0.17527329199999997,"d":"0.18"},{"v":1.1090864845776385,"d":"1.11"},{"v":1.1090864845776385,"d":"1.11"},{"v":0.6087962189999999,"d":"0.61"}]
["47153","Sequatchie","TN",{"v":0.176641939,"d":"0.18"},{"v":1.189084800121632,"d":"1.19"},{"v":1.1890848001216319,"d":"1.19"},{"v":0.5734420805000001,"d":"0.57"}]
["47155","Sevier","TN",{"v":0.159186902,"d":"0.16"},{"v":1.1698547409029436,"d":"1.17"},{"v":1.1698547409029436,"d":"1.17"},{"v":0.55887079,"d":"0.56"}]
["47157","Shelby","TN",{"v":0.108957086,"d":"0.11"},{"v":0.6359369740147566,"d":"0.64"},{"v":0.6359369740147566,"d":"0.64"},{"v":0.350766079,"d":"0.35"}]
["47159","Smith","TN",{"v":0.189977079,"d":"0.19"},{"v":1.138355581152852,"d":"1.14"},{"v":1.138355581152852,"d":"1.14"},{"v":0.496738462,"d":"0.50"}]
["47161","Stewart","TN",{"v":0.195423739,"d":"0.20"},{"v":1.1985921594514413,"d":"1.20"},{"v":1.1985921594514415,"d":"1.20"},{"v":0.5463894745,"d":"0.55"}]
["47163","Sullivan","TN",{"v":0.14754433100000003,"d":"0.15"},{"v":1.1339382484915326,"d":"1.13"},{"v":1.1339382484915326,"d":"1.13"},{"v":0.4350723839999999,"d":"0.44"}]
["47165","Sumner","TN",{"v":0.156666675,"d":"0.16"},{"v":1.0758796468057346,"d":"1.08"},{"v":1.0758796468057348,"d":"1.08"},{"v":0.40393690649999997,"d":"0.40"}]
["47167","Tipton","TN",{"v":0.18507831700000002,"d":"0.19"},{"v":1.0440312351898493,"d":"1.04"},{"v":1.0440312351898495,"d":"1.04"},{"v":0.41914371,"d":"0.42"}]
["47169","Trousdale","TN",{"v":0.203483852,"d":"0.20"},{"v":1.1494647582485273,"d":"1.15"},{"v":1.1494647582485273,"d":"1.15"},{"v":0.4783238460000001,"d":"0.48"}]
["47171","Unicoi","TN",{"v":0.157200201,"d":"0.16"},{"v":1.1520551014765987,"d":"1.15"},{"v":1.152055101476599,"d":"1.15"},{"v":0.575420795,"d":"0.58"}]
["47173","Union","TN",{"v":0.190092932,"d":"0.19"},{"v":1.2202749649020628,"d":"1.22"},{"v":1.2202749649020626,"d":"1.22"},{"v":0.5238725649999999,"d":"0.52"}]
["47175","Van Buren","TN",{"v":0.19097034999999998,"d":"0.19"},{"v":1.1958224873471925,"d":"1.20"},{"v":1.1958224873471925,"d":"1.20"},{"v":0.5693835730000001,"d":"0.57"}]
["47177","Warren","TN",{"v":0.179294395,"d":"0.18"},{"v":1.1216276584680813,"d":"1.12"},{"v":1.1216276584680813,"d":"1.12"},{"v":0.45975583800000003,"d":"0.46"}]
["47179","Washington","TN",{"v":0.150217082,"d":"0.15"},{"v":1.1065494580654578,"d":"1.11"},{"v":1.1065494580654578,"d":"1.11"},{"v":0.40137282150000003,"d":"0.40"}]
["47181","Wayne","TN",{"v":0.192959043,"d":"0.19"},{"v":1.1842063870530353,"d":"1.18"},{"v":1.184206387053035,"d":"1.18"},{"v":0.562233546,"d":"0.56"}]
["47183","Weakley","TN",{"v":0.193876578,"d":"0.19"},{"v":1.0977530232744075,"d":"1.10"},{"v":1.0977530232744075,"d":"1.10"},{"v":0.44223002,"d":"0.44"}]
["47185","White","TN",{"v":0.184952411,"d":"0.18"},{"v":1.1238741079519854,"d":"1.12"},{"v":1.1238741079519854,"d":"1.12"},{"v":0.512508099,"d":"0.51"}]
["47187","Williamson","TN",{"v":0.15112647299999998,"d":"0.15"},{"v":1.0442684568333924,"d":"1.04"},{"v":1.0442684568333922,"d":"1.04"},{"v":0.41807178149999996,"d":"0.42"}]
["47189","Wilson","TN",{"v":0.168674396,"d":"0.17"},{"v":1.0925137934367184,"d":"1.09"},{"v":1.0925137934367184,"d":"1.09"},{"v":0.417187725,"d":"0.42"}]
["48001","Anderson","TX",{"v":0.16064959100000004,"d":"0.16"},{"v":0.9273863352611732,"d":"0.93"},{"v":0.9273863352611733,"d":"0.93"},{"v":0.41930575750000004,"d":"0.42"}]
["48003","Andrews","TX",{"v":0.159483663,"d":"0.16"},{"v":0.9717315421502511,"d":"0.97"},{"v":0.9717315421502511,"d":"0.97"},{"v":0.2973401465,"d":"0.30"}]
["48005","Angelina","TX",{"v":0.149173378,"d":"0.15"},{"v":0.9146104879005239,"d":"0.91"},{"v":0.9146104879005239,"d":"0.91"},{"v":0.42556027049999995,"d":"0.43"}]
["48007","Aransas","TX",{"v":0.16728918,"d":"0.17"},{"v":0.8740534552705972,"d":"0.87"},{"v":0.874053455270597,"d":"0.87"},{"v":0.2901477635,"d":"0.29"}]
["48009","Archer","TX",{"v":0.20086401700000003,"d":"0.20"},{"v":0.9251945368084593,"d":"0.93"},{"v":0.9251945368084594,"d":"0.93"},{"v":0.3390809719999999,"d":"0.34"}]
["48011","Armstrong","TX",{"v":0.20020520300000003,"d":"0.20"},{"v":0.9214280289849601,"d":"0.92"},{"v":0.9214280289849601,"d":"0.92"},{"v":0.357430917,"d":"0.36"}]
["48013","Atascosa","TX",{"v":0.180182883,"d":"0.18"},{"v":0.8887902388147398,"d":"0.89"},{"v":0.88879023881474,"d":"0.89"},{"v":0.33716749349999997,"d":"0.34"}]
["48015","Austin","TX",{"v":0.185154976,"d":"0.19"},{"v":0.8810590550581223,"d":"0.88"},{"v":0.8810590550581223,"d":"0.88"},{"v":0.3485587614999999,"d":"0.35"}]
["48017","Bailey","TX",{"v":0.170218807,"d":"0.17"},{"v":0.9505994185681595,"d":"0.95"},{"v":0.9505994185681597,"d":"0.95"},{"v":0.3024346745,"d":"0.30"}]
["48019","Bandera","TX",{"v":0.184577881,"d":"0.18"},{"v":0.9720873552841273,"d":"0.97"},{"v":0.972087355284127,"d":"0.97"},{"v":0.42179656549999994,"d":"0.42"}]
["48021","Bastrop","TX",{"v":0.17303830299999998,"d":"0.17"},{"v":0.8988010118173022,"d":"0.90"},{"v":0.8988010118173022,"d":"0.90"},{"v":0.371786593,"d":"0.37"}]
["48023","Baylor","TX",{"v":0.204155112,"d":"0.20"},{"v":0.8866737704774331,"d":"0.89"},{"v":0.8866737704774331,"d":"0.89"},{"v":0.35132085900000004,"d":"0.35"}]
["48025","Bee","TX",{"v":0.172439911,"d":"0.17"},{"v":0.8661158840213274,"d":"0.87"},{"v":0.8661158840213274,"d":"0.87"},{"v":0.32902939649999996,"d":"0.33"}]
["48027","Bell","TX",{"v":0.14342125799999997,"d":"0.14"},{"v":0.8998166986652906,"d":"0.90"},{"v":0.8998166986652906,"d":"0.90"},{"v":0.30967845200000005,"d":"0.31"}]
["48029","Bexar","TX",{"v":0.092909501,"d":"0.09"},{"v":0.40979426207022673,"d":"0.41"},{"v":0.4097942620702267,"d":"0.41"},{"v":0.27222270900000006,"d":"0.27"}]
["48031","Blanco","TX",{"v":0.195622929,"d":"0.20"},{"v":0.9451514980192484,"d":"0.95"},{"v":0.9451514980192484,"d":"0.95"},{"v":0.384629415,"d":"0.38"}]
["48033","Borden","TX",{"v":0.20398666500000004,"d":"0.20"},{"v":0.9772845843072772,"d":"0.98"},{"v":0.9772845843072772,"d":"0.98"},{"v":0.3500903995,"d":"0.35"}]
["48035","Bosque","TX",{"v":0.185358238,"d":"0.19"},{"v":0.932398700720561,"d":"0.93"},{"v":0.932398700720561,"d":"0.93"},{"v":0.3797562939999999,"d":"0.38"}]
["48037","Bowie","TX",{"v":0.152222361,"d":"0.15"},{"v":0.8817983696674232,"d":"0.88"},{"v":0.8817983696674231,"d":"0.88"},{"v":0.37834939249999994,"d":"0.38"}]
["48039","Brazoria","TX",{"v":0.150551312,"d":"0.15"},{"v":0.8294880879697621,"d":"0.83"},{"v":0.8294880879697621,"d":"0.83"},{"v":0.2975641775,"d":"0.30"}]
["48041","Brazos","TX",{"v":0.135224811,"d":"0.14"},{"v":0.8456140309816611,"d":"0.85"},{"v":0.8456140309816611,"d":"0.85"},{"v":0.3183492505,"d":"0.32"}]
["48043","Brewster","TX",{"v":0.17030577399999997,"d":"0.17"},{"v":0.888116193407746,"d":"0.89"},{"v":0.8881161934077461,"d":"0.89"},{"v":0.3160501005,"d":"0.32"}]
["48045","Briscoe","TX",{"v":0.197962535,"d":"0.20"},{"v":0.9152388607489452,"d":"0.92"},{"v":0.9152388607489452,"d":"0.92"},{"v":0.363494112,"d":"0.36"}]
["48047","Brooks","TX",{"v":0.172769422,"d":"0.17"},{"v":0.8555932032386891,"d":"0.86"},{"v":0.8555932032386891,"d":"0.86"},{"v":0.3139698965,"d":"0.31"}]
["48049","Brown","TX",{"v":0.165971235,"d":"0.17"},{"v":0.9154536754253764,"d":"0.92"},{"v":0.9154536754253764,"d":"0.92"},{"v":0.3462666525,"d":"0.35"}]
["48051","Burleson","TX",{"v":0.18583955499999996,"d":"0.19"},{"v":0.910051350249508,"d":"0.91"},{"v":0.910051350249508,"d":"0.91"},{"v":0.36510675300000006,"d":"0.37"}]
["48053","Burnet","TX",{"v":0.17509613499999999,"d":"0.18"},{"v":0.9359871176853952,"d":"0.94"},{"v":0.9359871176853952,"d":"0.94"},{"v":0.36237942549999996,"d":"0.36"}]
["48055","Caldwell","TX",{"v":0.16919708,"d":"0.17"},{"v":0.8766896404227609,"d":"0.88"},{"v":0.8766896404227609,"d":"0.88"},{"v":0.34251423,"d":"0.34"}]
["48057","Calhoun","TX",{"v":0.18422286000000002,"d":"0.18"},{"v":0.8652117983815553,"d":"0.87"},{"v":0.8652117983815553,"d":"0.87"},{"v":0.3044714415,"d":"0.30"}]
["48059","Callahan","TX",{"v":0.183451596,"d":"0.18"},{"v":0.9461569248058328,"d":"0.95"},{"v":0.946156924805833,"d":"0.95"},{"v":0.35809121800000004,"d":"0.36"}]
["48061","Cameron","TX",{"v":0.144701499,"d":"0.14"},{"v":0.8287415847988624,"d":"0.83"},{"v":0.8287415847988623,"d":"0.83"},{"v":0.257834134,"d":"0.26"}]
["48063","Camp","TX",{"v":0.168146086,"d":"0.17"},{"v":0.9125163800616768,"d":"0.91"},{"v":0.9125163800616768,"d":"0.91"},{"v":0.40278279250000004,"d":"0.40"}]
["48065","Carson","TX",{"v":0.20031865499999998,"d":"0.20"},{"v":0.925974551120338,"d":"0.93"},{"v":0.9259745511203381,"d":"0.93"},{"v":0.34367222199999997,"d":"0.34"}]
["48067","Cass","TX",{"v":0.16793209,"d":"0.17"},{"v":0.9191055783750415,"d":"0.92"},{"v":0.9191055783750413,"d":"0.92"},{"v":0.456439992,"d":"0.46"}]
["48069","Castro","TX",{"v":0.178482829,"d":"0.18"},{"v":0.9158404478113717,"d":"0.92"},{"v":0.9158404478113719,"d":"0.92"},{"v":0.315286298,"d":"0.32"}]
["48071","Chambers","TX",{"v":0.177512958,"d":"0.18"},{"v":0.8704162478947982,"d":"0.87"},{"v":0.8704162478947981,"d":"0.87"},{"v":0.31372126199999995,"d":"0.31"}]
["48073","Cherokee","TX",{"v":0.164626897,"d":"0.16"},{"v":0.9082607813806626,"d":"0.91"},{"v":0.9082607813806626,"d":"0.91"},{"v":0.4324331315,"d":"0.43"}]
["48075","Childress","TX",{"v":0.166285492,"d":"0.17"},{"v":0.9011119781259394,"d":"0.90"},{"v":0.9011119781259394,"d":"0.90"},{"v":0.2975358575,"d":"0.30"}]
["48077","Clay","TX",{"v":0.19117612,"d":"0.19"},{"v":0.9309780618375977,"d":"0.93"},{"v":0.9309780618375977,"d":"0.93"},{"v":0.33946031950000005,"d":"0.34"}]
["48079","Cochran","TX",{"v":0.20347292000000003,"d":"0.20"},{"v":0.9057341583436238,"d":"0.91"},{"v":0.9057341583436237,"d":"0.91"},{"v":0.3465380725,"d":"0.35"}]
["48081","Coke","TX",{"v":0.196466427,"d":"0.20"},{"v":0.918901933133686,"d":"0.92"},{"v":0.918901933133686,"d":"0.92"},{"v":0.376417987,"d":"0.38"}]
["48083","Coleman","TX",{"v":0.175124323,"d":"0.18"},{"v":0.91067530988849,"d":"0.91"},{"v":0.9106753098884899,"d":"0.91"},{"v":0.34416545000000004,"d":"0.34"}]
["48085","Collin","TX",{"v":0.107273217,"d":"0.11"},{"v":0.672528580430149,"d":"0.67"},{"v":0.672528580430149,"d":"0.67"},{"v":0.26803778149999996,"d":"0.27"}]
["48087","Collingsworth","TX",{"v":0.204917967,"d":"0.20"},{"v":0.873192393146278,"d":"0.87"},{"v":0.8731923931462778,"d":"0.87"},{"v":0.3498898014999999,"d":"0.35"}]
["48089","Colorado","TX",{"v":0.180746415,"d":"0.18"},{"v":0.8741073916323746,"d":"0.87"},{"v":0.8741073916323746,"d":"0.87"},{"v":0.356444446,"d":"0.36"}]
["48091","Comal","TX",{"v":0.15555500899999997,"d":"0.16"},{"v":0.8790137793372234,"d":"0.88"},{"v":0.8790137793372235,"d":"0.88"},{"v":0.36073581949999994,"d":"0.36"}]
["48093","Comanche","TX",{"v":0.181681697,"d":"0.18"},{"v":0.9391263509603448,"d":"0.94"},{"v":0.9391263509603449,"d":"0.94"},{"v":0.364009437,"d":"0.36"}]
["48095","Concho","TX",{"v":0.205407431,"d":"0.21"},{"v":0.904106020899755,"d":"0.90"},{"v":0.9041060208997551,"d":"0.90"},{"v":0.35092363449999997,"d":"0.35"}]
["48097","Cooke","TX",{"v":0.17772227700000004,"d":"0.18"},{"v":0.9199300336563961,"d":"0.92"},{"v":0.9199300336563961,"d":"0.92"},{"v":0.34702804649999996,"d":"0.35"}]
["48099","Coryell","TX",{"v":0.163116798,"d":"0.16"},{"v":0.9060209493133489,"d":"0.91"},{"v":0.9060209493133489,"d":"0.91"},{"v":0.334844255,"d":"0.33"}]
["48101","Cottle","TX",{"v":0.201611494,"d":"0.20"},{"v":0.852348458606588,"d":"0.85"},{"v":0.852348458606588,"d":"0.85"},{"v":0.3647786484999999,"d":"0.36"}]
["48103","Crane","TX",{"v":0.164631522,"d":"0.16"},{"v":0.887943473354699,"d":"0.89"},{"v":0.8879434733546989,"d":"0.89"},{"v":0.28253695649999994,"d":"0.28"}]
["48105","Crockett","TX",{"v":0.167716695,"d":"0.17"},{"v":0.8926426890495972,"d":"0.89"},{"v":0.8926426890495972,"d":"0.89"},{"v":0.313120435,"d":"0.31"}]
["48107","Crosby","TX",{"v":0.203320145,"d":"0.20"},{"v":0.910505253807223,"d":"0.91"},{"v":0.910505253807223,"d":"0.91"},{"v":0.3531939755,"d":"0.35"}]
["48109","Culberson","TX",{"v":0.205605878,"d":"0.21"},{"v":0.843175747728722,"d":"0.84"},{"v":0.8431757477287221,"d":"0.84"},{"v":0.342905864,"d":"0.34"}]
["48111","Dallam","TX",{"v":0.165890265,"d":"0.17"},{"v":0.9260302227694204,"d":"0.93"},{"v":0.9260302227694204,"d":"0.93"},{"v":0.29893323600000005,"d":"0.30"}]
["48113","Dallas","TX",{"v":0.056202853,"d":"0.06"},{"v":0.00396220932772887,"d":"0.00"},{"v":0.00396220932772887,"d":"0.00"},{"v":0.23184839799999998,"d":"0.23"}]
["48115","Dawson","TX",{"v":0.162808782,"d":"0.16"},{"v":0.9150984713618234,"d":"0.92"},{"v":0.9150984713618232,"d":"0.92"},{"v":0.29632090800000005,"d":"0.30"}]
["48117","Deaf Smith","TX",{"v":0.163771314,"d":"0.16"},{"v":0.9082997223802985,"d":"0.91"},{"v":0.9082997223802985,"d":"0.91"},{"v":0.292989444,"d":"0.29"}]
["48119","Delta","TX",{"v":0.19948872299999998,"d":"0.20"},{"v":0.9219344144813727,"d":"0.92"},{"v":0.9219344144813727,"d":"0.92"},{"v":0.3711421045,"d":"0.37"}]
["48121","Denton","TX",{"v":0.115632188,"d":"0.12"},{"v":0.7754174927587698,"d":"0.78"},{"v":0.7754174927587698,"d":"0.78"},{"v":0.26917413349999997,"d":"0.27"}]
["48123","De Witt","TX",{"v":0.177188241,"d":"0.18"},{"v":0.8681641349037191,"d":"0.87"},{"v":0.8681641349037191,"d":"0.87"},{"v":0.35102952350000005,"d":"0.35"}]
["48125","Dickens","TX",{"v":0.200757158,"d":"0.20"},{"v":0.9519405909092208,"d":"0.95"},{"v":0.951940590909221,"d":"0.95"},{"v":0.3619570690000001,"d":"0.36"}]
["48127","Dimmit","TX",{"v":0.179140105,"d":"0.18"},{"v":0.8662256319621773,"d":"0.87"},{"v":0.8662256319621773,"d":"0.87"},{"v":0.313381962,"d":"0.31"}]
["48129","Donley","TX",{"v":0.20212978800000003,"d":"0.20"},{"v":0.9075505794001868,"d":"0.91"},{"v":0.9075505794001869,"d":"0.91"},{"v":0.3540446795,"d":"0.35"}]
["48131","Duval","TX",{"v":0.187992271,"d":"0.19"},{"v":0.8609251689705381,"d":"0.86"},{"v":0.860925168970538,"d":"0.86"},{"v":0.346224389,"d":"0.35"}]
["48133","Eastland","TX",{"v":0.176276025,"d":"0.18"},{"v":0.9186499340554591,"d":"0.92"},{"v":0.9186499340554591,"d":"0.92"},{"v":0.36378062,"d":"0.36"}]
["48135","Ector","TX",{"v":0.14935728700000003,"d":"0.15"},{"v":0.8890849237260042,"d":"0.89"},{"v":0.8890849237260041,"d":"0.89"},{"v":0.2740289605,"d":"0.27"}]
["48137","Edwards","TX",{"v":0.194814364,"d":"0.19"},{"v":0.9524553982578664,"d":"0.95"},{"v":0.9524553982578665,"d":"0.95"},{"v":0.38449486749999995,"d":"0.38"}]
["48139","Ellis","TX",{"v":0.15921751100000003,"d":"0.16"},{"v":0.9166375960958287,"d":"0.92"},{"v":0.9166375960958288,"d":"0.92"},{"v":0.31562263,"d":"0.32"}]
["48141","El Paso","TX",{"v":0.12091586600000001,"d":"0.12"},{"v":0.7489397375358869,"d":"0.75"},{"v":0.7489397375358868,"d":"0.75"},{"v":0.2566261955,"d":"0.26"}]
["48143","Erath","TX",{"v":0.164038209,"d":"0.16"},{"v":0.9389172208146948,"d":"0.94"},{"v":0.9389172208146948,"d":"0.94"},{"v":0.3495235075,"d":"0.35"}]
["48145","Falls","TX",{"v":0.183096422,"d":"0.18"},{"v":0.9125871875657776,"d":"0.91"},{"v":0.9125871875657776,"d":"0.91"},{"v":0.33829837799999996,"d":"0.34"}]
["48147","Fannin","TX",{"v":0.18225025899999997,"d":"0.18"},{"v":0.9216074296500368,"d":"0.92"},{"v":0.9216074296500367,"d":"0.92"},{"v":0.36706408749999997,"d":"0.37"}]
["48149","Fayette","TX",{"v":0.184753483,"d":"0.18"},{"v":0.8820129301511199,"d":"0.88"},{"v":0.88201293015112,"d":"0.88"},{"v":0.35066337150000004,"d":"0.35"}]
["48151","Fisher","TX",{"v":0.199163711,"d":"0.20"},{"v":0.8966784194200549,"d":"0.90"},{"v":0.896678419420055,"d":"0.90"},{"v":0.36738346650000003,"d":"0.37"}]
["48153","Floyd","TX",{"v":0.180376712,"d":"0.18"},{"v":0.9103074062785963,"d":"0.91"},{"v":0.9103074062785963,"d":"0.91"},{"v":0.3240540805,"d":"0.32"}]
["48155","Foard","TX",{"v":0.20133163000000004,"d":"0.20"},{"v":0.8883123178954767,"d":"0.89"},{"v":0.8883123178954766,"d":"0.89"},{"v":0.3652655729999999,"d":"0.37"}]
["48157","Fort Bend","TX",{"v":0.124347974,"d":"0.12"},{"v":0.740006714483981,"d":"0.74"},{"v":0.740006714483981,"d":"0.74"},{"v":0.2700391195,"d":"0.27"}]
["48159","Franklin","TX",{"v":0.176370456,"d":"0.18"},{"v":0.9149682502315161,"d":"0.91"},{"v":0.9149682502315161,"d":"0.91"},{"v":0.384431338,"d":"0.38"}]
["48161","Freestone","TX",{"v":0.173663811,"d":"0.17"},{"v":0.9378299968120175,"d":"0.94"},{"v":0.9378299968120175,"d":"0.94"},{"v":0.38116090899999994,"d":"0.38"}]
["48163","Frio","TX",{"v":0.16879734900000004,"d":"0.17"},{"v":0.8734635878963585,"d":"0.87"},{"v":0.8734635878963585,"d":"0.87"},{"v":0.318056642,"d":"0.32"}]
["48165","Gaines","TX",{"v":0.181425298,"d":"0.18"},{"v":0.9702648901575656,"d":"0.97"},{"v":0.9702648901575656,"d":"0.97"},{"v":0.3286372245,"d":"0.33"}]
["48167","Galveston","TX",{"v":0.124405635,"d":"0.12"},{"v":0.7147086972163046,"d":"0.71"},{"v":0.7147086972163046,"d":"0.71"},{"v":0.24986760400000005,"d":"0.25"}]
["48169","Garza","TX",{"v":0.169254278,"d":"0.17"},{"v":0.8983077190749377,"d":"0.90"},{"v":0.8983077190749377,"d":"0.90"},{"v":0.314829389,"d":"0.31"}]
["48171","Gillespie","TX",{"v":0.17077935099999997,"d":"0.17"},{"v":0.911498135416356,"d":"0.91"},{"v":0.9114981354163562,"d":"0.91"},{"v":0.36938080600000006,"d":"0.37"}]
["48173","Glasscock","TX",{"v":0.202780603,"d":"0.20"},{"v":1.002584583376256,"d":"1.00"},{"v":1.002584583376256,"d":"1.00"},{"v":0.3534129935000001,"d":"0.35"}]
["48175","Goliad","TX",{"v":0.19971966500000005,"d":"0.20"},{"v":0.894964727465972,"d":"0.89"},{"v":0.8949647274659718,"d":"0.89"},{"v":0.375818653,"d":"0.38"}]
["48177","Gonzales","TX",{"v":0.183296434,"d":"0.18"},{"v":0.8873789309157398,"d":"0.89"},{"v":0.8873789309157398,"d":"0.89"},{"v":0.3565975995,"d":"0.36"}]
["48179","Gray","TX",{"v":0.16119815099999998,"d":"0.16"},{"v":0.9004775505129697,"d":"0.90"},{"v":0.9004775505129697,"d":"0.90"},{"v":0.29384461000000006,"d":"0.29"}]
["48181","Grayson","TX",{"v":0.16092607100000003,"d":"0.16"},{"v":0.8925521998341217,"d":"0.89"},{"v":0.8925521998341216,"d":"0.89"},{"v":0.33985021350000005,"d":"0.34"}]
["48183","Gregg","TX",{"v":0.126844459,"d":"0.13"},{"v":0.8467308342455976,"d":"0.85"},{"v":0.8467308342455976,"d":"0.85"},{"v":0.355923477,"d":"0.36"}]
["48185","Grimes","TX",{"v":0.17676909800000004,"d":"0.18"},{"v":0.9389487471465802,"d":"0.94"},{"v":0.93894874714658,"d":"0.94"},{"v":0.38529030050000007,"d":"0.39"}]
["48187","Guadalupe","TX",{"v":0.155851194,"d":"0.16"},{"v":0.8865106443760299,"d":"0.89"},{"v":0.8865106443760301,"d":"0.89"},{"v":0.3157839475,"d":"0.32"}]
["48189","Hale","TX",{"v":0.16771238599999996,"d":"0.17"},{"v":0.9067511383429568,"d":"0.91"},{"v":0.9067511383429568,"d":"0.91"},{"v":0.2991346860000001,"d":"0.30"}]
["48191","Hall","TX",{"v":0.20512045499999998,"d":"0.21"},{"v":0.8576437162170478,"d":"0.86"},{"v":0.8576437162170478,"d":"0.86"},{"v":0.35435423,"d":"0.35"}]
["48193","Hamilton","TX",{"v":0.18195445199999996,"d":"0.18"},{"v":0.9057008540149523,"d":"0.91"},{"v":0.9057008540149523,"d":"0.91"},{"v":0.35295058499999993,"d":"0.35"}]
["48195","Hansford","TX",{"v":0.175170113,"d":"0.18"},{"v":0.9006521820798409,"d":"0.90"},{"v":0.9006521820798409,"d":"0.90"},{"v":0.31293673349999995,"d":"0.31"}]
["48197","Hardeman","TX",{"v":0.202278303,"d":"0.20"},{"v":0.8744465690849313,"d":"0.87"},{"v":0.8744465690849313,"d":"0.87"},{"v":0.3563044025,"d":"0.36"}]
["48199","Hardin","TX",{"v":0.149457198,"d":"0.15"},{"v":0.9517124252194712,"d":"0.95"},{"v":0.9517124252194711,"d":"0.95"},{"v":0.46413479050000017,"d":"0.46"}]
["48201","Harris","TX",{"v":0.063488635,"d":"0.06"},{"v":0.01254523198512237,"d":"0.01"},{"v":0.012545231985122371,"d":"0.01"},{"v":0.23901160300000002,"d":"0.24"}]
["48203","Harrison","TX",{"v":0.159002394,"d":"0.16"},{"v":0.9099862410129175,"d":"0.91"},{"v":0.9099862410129176,"d":"0.91"},{"v":0.4263735685000001,"d":"0.43"}]
["48205","Hartley","TX",{"v":0.174234036,"d":"0.17"},{"v":0.9353899971216858,"d":"0.94"},{"v":0.9353899971216856,"d":"0.94"},{"v":0.31253920649999994,"d":"0.31"}]
["48207","Haskell","TX",{"v":0.180049015,"d":"0.18"},{"v":0.9055424752802915,"d":"0.91"},{"v":0.9055424752802915,"d":"0.91"},{"v":0.327860121,"d":"0.33"}]
["48209","Hays","TX",{"v":0.145409646,"d":"0.15"},{"v":0.8600664649433952,"d":"0.86"},{"v":0.8600664649433951,"d":"0.86"},{"v":0.34482543400000004,"d":"0.34"}]
["48211","Hemphill","TX",{"v":0.16372692,"d":"0.16"},{"v":0.9217795364638556,"d":"0.92"},{"v":0.9217795364638557,"d":"0.92"},{"v":0.3111829440000001,"d":"0.31"}]
["48213","Henderson","TX",{"v":0.167843933,"d":"0.17"},{"v":0.9485772327314169,"d":"0.95"},{"v":0.9485772327314169,"d":"0.95"},{"v":0.37526764599999995,"d":"0.38"}]
["48215","Hidalgo","TX",{"v":0.141063226,"d":"0.14"},{"v":0.8320831934675943,"d":"0.83"},{"v":0.8320831934675943,"d":"0.83"},{"v":0.25917913200000003,"d":"0.26"}]
["48217","Hill","TX",{"v":0.186879063,"d":"0.19"},{"v":0.9415507180074045,"d":"0.94"},{"v":0.9415507180074045,"d":"0.94"},{"v":0.35305349599999997,"d":"0.35"}]
["48219","Hockley","TX",{"v":0.170198917,"d":"0.17"},{"v":0.930202610543547,"d":"0.93"},{"v":0.930202610543547,"d":"0.93"},{"v":0.313417109,"d":"0.31"}]
["48221","Hood","TX",{"v":0.157803981,"d":"0.16"},{"v":0.9596012373172877,"d":"0.96"},{"v":0.9596012373172877,"d":"0.96"},{"v":0.32797828500000004,"d":"0.33"}]
["48223","Hopkins","TX",{"v":0.172989593,"d":"0.17"},{"v":0.913727555445728,"d":"0.91"},{"v":0.9137275554457281,"d":"0.91"},{"v":0.35608015249999997,"d":"0.36"}]
["48225","Houston","TX",{"v":0.171122327,"d":"0.17"},{"v":0.9120732969129901,"d":"0.91"},{"v":0.9120732969129903,"d":"0.91"},{"v":0.4201924595,"d":"0.42"}]
["48227","Howard","TX",{"v":0.16010116099999996,"d":"0.16"},{"v":0.9310052108552812,"d":"0.93"},{"v":0.9310052108552813,"d":"0.93"},{"v":0.30965890600000007,"d":"0.31"}]
["48229","Hudspeth","TX",{"v":0.20779719399999996,"d":"0.21"},{"v":0.9554408808576142,"d":"0.96"},{"v":0.9554408808576142,"d":"0.96"},{"v":0.33841576450000005,"d":"0.34"}]
["48231","Hunt","TX",{"v":0.167136663,"d":"0.17"},{"v":0.9303866227257148,"d":"0.93"},{"v":0.9303866227257148,"d":"0.93"},{"v":0.34533487150000003,"d":"0.35"}]
["48233","Hutchinson","TX",{"v":0.164083661,"d":"0.16"},{"v":0.9126581265077225,"d":"0.91"},{"v":0.9126581265077226,"d":"0.91"},{"v":0.30030798899999994,"d":"0.30"}]
["48235","Irion","TX",{"v":0.206679336,"d":"0.21"},{"v":0.9327855181533179,"d":"0.93"},{"v":0.9327855181533178,"d":"0.93"},{"v":0.3496470809999999,"d":"0.35"}]
["48237","Jack","TX",{"v":0.17645756199999998,"d":"0.18"},{"v":0.9147378380039376,"d":"0.91"},{"v":0.9147378380039376,"d":"0.91"},{"v":0.3639018704999999,"d":"0.36"}]
["48239","Jackson","TX",{"v":0.183225425,"d":"0.18"},{"v":0.8770041762169303,"d":"0.88"},{"v":0.8770041762169303,"d":"0.88"},{"v":0.3366634385,"d":"0.34"}]
["48241","Jasper","TX",{"v":0.16575450899999997,"d":"0.17"},{"v":0.951107243299718,"d":"0.95"},{"v":0.9511072432997181,"d":"0.95"},{"v":0.47334044850000007,"d":"0.47"}]
["48243","Jeff Davis","TX",{"v":0.20543663300000004,"d":"0.21"},{"v":0.9202973688315798,"d":"0.92"},{"v":0.9202973688315798,"d":"0.92"},{"v":0.3507304279999999,"d":"0.35"}]
["48245","Jefferson","TX",{"v":0.146942297,"d":"0.15"},{"v":0.8166148283881975,"d":"0.82"},{"v":0.8166148283881975,"d":"0.82"},{"v":0.275320658,"d":"0.28"}]
["48247","Jim Hogg","TX",{"v":0.169489566,"d":"0.17"},{"v":0.8290502307097986,"d":"0.83"},{"v":0.8290502307097984,"d":"0.83"},{"v":0.29680154599999997,"d":"0.30"}]
["48249","Jim Wells","TX",{"v":0.173544886,"d":"0.17"},{"v":0.8515439625271752,"d":"0.85"},{"v":0.8515439625271752,"d":"0.85"},{"v":0.32003612800000003,"d":"0.32"}]
["48251","Johnson","TX",{"v":0.15777228799999998,"d":"0.16"},{"v":0.9378204167590776,"d":"0.94"},{"v":0.9378204167590776,"d":"0.94"},{"v":0.32367982050000005,"d":"0.32"}]
["48253","Jones","TX",{"v":0.191471981,"d":"0.19"},{"v":0.9375313909744548,"d":"0.94"},{"v":0.9375313909744549,"d":"0.94"},{"v":0.34545630150000006,"d":"0.35"}]
["48255","Karnes","TX",{"v":0.17739759599999996,"d":"0.18"},{"v":0.8666495398528145,"d":"0.87"},{"v":0.8666495398528145,"d":"0.87"},{"v":0.3321840325,"d":"0.33"}]
["48257","Kaufman","TX",{"v":0.168096794,"d":"0.17"},{"v":0.9263719833740172,"d":"0.93"},{"v":0.926371983374017,"d":"0.93"},{"v":0.3349794735,"d":"0.33"}]
["48259","Kendall","TX",{"v":0.16738861300000002,"d":"0.17"},{"v":0.9249009978475297,"d":"0.92"},{"v":0.9249009978475297,"d":"0.92"},{"v":0.37692729199999997,"d":"0.38"}]
["48261","Kenedy","TX",{"v":0.21628326000000003,"d":"0.22"},{"v":0.8802126771805763,"d":"0.88"},{"v":0.8802126771805762,"d":"0.88"},{"v":0.33520895200000006,"d":"0.34"}]
["48263","Kent","TX",{"v":0.19906110900000004,"d":"0.20"},{"v":0.9818846913333102,"d":"0.98"},{"v":0.9818846913333102,"d":"0.98"},{"v":0.367444209,"d":"0.37"}]
["48265","Kerr","TX",{"v":0.160213168,"d":"0.16"},{"v":0.9282058702755172,"d":"0.93"},{"v":0.9282058702755172,"d":"0.93"},{"v":0.37370220750000005,"d":"0.37"}]
["48267","Kimble","TX",{"v":0.169536375,"d":"0.17"},{"v":0.9133058384759603,"d":"0.91"},{"v":0.9133058384759603,"d":"0.91"},{"v":0.3615228885,"d":"0.36"}]
["48269","King","TX",{"v":0.19783338700000003,"d":"0.20"},{"v":0.9746907003026305,"d":"0.97"},{"v":0.9746907003026305,"d":"0.97"},{"v":0.368515653,"d":"0.37"}]
["48271","Kinney","TX",{"v":0.167169177,"d":"0.17"},{"v":0.9260267698721275,"d":"0.93"},{"v":0.9260267698721274,"d":"0.93"},{"v":0.305992168,"d":"0.31"}]
["48273","Kleberg","TX",{"v":0.169885639,"d":"0.17"},{"v":0.8592418211878483,"d":"0.86"},{"v":0.8592418211878483,"d":"0.86"},{"v":0.2845410115,"d":"0.28"}]
["48275","Knox","TX",{"v":0.202834151,"d":"0.20"},{"v":0.8670272827476188,"d":"0.87"},{"v":0.8670272827476189,"d":"0.87"},{"v":0.3628109845,"d":"0.36"}]
["48277","Lamar","TX",{"v":0.16596363400000003,"d":"0.17"},{"v":0.9124585176303056,"d":"0.91"},{"v":0.9124585176303056,"d":"0.91"},{"v":0.3515738005,"d":"0.35"}]
["48279","Lamb","TX",{"v":0.18409787599999997,"d":"0.18"},{"v":0.9178424102773218,"d":"0.92"},{"v":0.9178424102773218,"d":"0.92"},{"v":0.322214059,"d":"0.32"}]
["48281","Lampasas","TX",{"v":0.18087640400000002,"d":"0.18"},{"v":0.9128106943888279,"d":"0.91"},{"v":0.9128106943888278,"d":"0.91"},{"v":0.355629583,"d":"0.36"}]
["48283","La Salle","TX",{"v":0.172110357,"d":"0.17"},{"v":0.878719947038074,"d":"0.88"},{"v":0.8787199470380741,"d":"0.88"},{"v":0.3146675895,"d":"0.31"}]
["48285","Lavaca","TX",{"v":0.1888247,"d":"0.19"},{"v":0.8768249317487874,"d":"0.88"},{"v":0.8768249317487875,"d":"0.88"},{"v":0.369460041,"d":"0.37"}]
["48287","Lee","TX",{"v":0.18765135900000002,"d":"0.19"},{"v":0.8963123821581102,"d":"0.90"},{"v":0.8963123821581103,"d":"0.90"},{"v":0.3558956745,"d":"0.36"}]
["48289","Leon","TX",{"v":0.18641872099999998,"d":"0.19"},{"v":0.9493488608682715,"d":"0.95"},{"v":0.9493488608682716,"d":"0.95"},{"v":0.417509057,"d":"0.42"}]
["48291","Liberty","TX",{"v":0.166201838,"d":"0.17"},{"v":0.8992064577517496,"d":"0.90"},{"v":0.8992064577517497,"d":"0.90"},{"v":0.409710812,"d":"0.41"}]
["48293","Limestone","TX",{"v":0.17711061899999997,"d":"0.18"},{"v":0.9326385078669387,"d":"0.93"},{"v":0.9326385078669387,"d":"0.93"},{"v":0.35156408050000004,"d":"0.35"}]
["48295","Lipscomb","TX",{"v":0.206010752,"d":"0.21"},{"v":0.9203577005767398,"d":"0.92"},{"v":0.9203577005767398,"d":"0.92"},{"v":0.3433274504999999,"d":"0.34"}]
["48297","Live Oak","TX",{"v":0.20263088,"d":"0.20"},{"v":0.8903105830975839,"d":"0.89"},{"v":0.890310583097584,"d":"0.89"},{"v":0.3638561455,"d":"0.36"}]
["48299","Llano","TX",{"v":0.170140607,"d":"0.17"},{"v":0.9297649944738717,"d":"0.93"},{"v":0.9297649944738717,"d":"0.93"},{"v":0.3550114025,"d":"0.36"}]
["48301","Loving","TX",{"v":0.19744712599999997,"d":"0.20"},{"v":0.9907355853000419,"d":"0.99"},{"v":0.9907355853000419,"d":"0.99"},{"v":0.34308823199999994,"d":"0.34"}]
["48303","Lubbock","TX",{"v":0.141830873,"d":"0.14"},{"v":0.9076464541409782,"d":"0.91"},{"v":0.9076464541409783,"d":"0.91"},{"v":0.2784277645,"d":"0.28"}]
["48305","Lynn","TX",{"v":0.18080766000000004,"d":"0.18"},{"v":0.9392696946478419,"d":"0.94"},{"v":0.9392696946478419,"d":"0.94"},{"v":0.3246792834999999,"d":"0.32"}]
["48307","McCulloch","TX",{"v":0.170566236,"d":"0.17"},{"v":0.8692743222562307,"d":"0.87"},{"v":0.8692743222562307,"d":"0.87"},{"v":0.335792742,"d":"0.34"}]
["48309","McLennan","TX",{"v":0.149265391,"d":"0.15"},{"v":0.8899390866753152,"d":"0.89"},{"v":0.8899390866753152,"d":"0.89"},{"v":0.311446065,"d":"0.31"}]
["48311","McMullen","TX",{"v":0.20267599700000002,"d":"0.20"},{"v":0.8745874317201049,"d":"0.87"},{"v":0.874587431720105,"d":"0.87"},{"v":0.36258897149999997,"d":"0.36"}]
["48313","Madison","TX",{"v":0.176915111,"d":"0.18"},{"v":0.9244233071442343,"d":"0.92"},{"v":0.9244233071442344,"d":"0.92"},{"v":0.363673919,"d":"0.36"}]
["48315","Marion","TX",{"v":0.17524441899999998,"d":"0.18"},{"v":0.9464830553905565,"d":"0.95"},{"v":0.9464830553905565,"d":"0.95"},{"v":0.46540025049999995,"d":"0.47"}]
["48317","Martin","TX",{"v":0.20225935100000003,"d":"0.20"},{"v":0.9704931525131877,"d":"0.97"},{"v":0.9704931525131877,"d":"0.97"},{"v":0.35156063,"d":"0.35"}]
["48319","Mason","TX",{"v":0.19669309499999996,"d":"0.20"},{"v":0.9393443625821728,"d":"0.94"},{"v":0.9393443625821726,"d":"0.94"},{"v":0.384562145,"d":"0.38"}]
["48321","Matagorda","TX",{"v":0.173878375,"d":"0.17"},{"v":0.8706070245366585,"d":"0.87"},{"v":0.8706070245366586,"d":"0.87"},{"v":0.30582802299999995,"d":"0.31"}]
["48323","Maverick","TX",{"v":0.16981904100000003,"d":"0.17"},{"v":0.8523947802727986,"d":"0.85"},{"v":0.8523947802727985,"d":"0.85"},{"v":0.26974034699999994,"d":"0.27"}]
["48325","Medina","TX",{"v":0.175641434,"d":"0.18"},{"v":0.9094677147120073,"d":"0.91"},{"v":0.9094677147120072,"d":"0.91"},{"v":0.3615831335,"d":"0.36"}]
["48327","Menard","TX",{"v":0.20224197399999996,"d":"0.20"},{"v":0.931596861574269,"d":"0.93"},{"v":0.9315968615742688,"d":"0.93"},{"v":0.36903030500000006,"d":"0.37"}]
["48329","Midland","TX",{"v":0.147289862,"d":"0.15"},{"v":0.9385003397804225,"d":"0.94"},{"v":0.9385003397804225,"d":"0.94"},{"v":0.2890345875,"d":"0.29"}]
["48331","Milam","TX",{"v":0.175840957,"d":"0.18"},{"v":0.9220730825860682,"d":"0.92"},{"v":0.9220730825860682,"d":"0.92"},{"v":0.35273160350000005,"d":"0.35"}]
["48333","Mills","TX",{"v":0.19636515800000004,"d":"0.20"},{"v":0.9218617956635959,"d":"0.92"},{"v":0.9218617956635959,"d":"0.92"},{"v":0.3805551755,"d":"0.38"}]
["48335","Mitchell","TX",{"v":0.17620088600000003,"d":"0.18"},{"v":0.9228451161260476,"d":"0.92"},{"v":0.9228451161260478,"d":"0.92"},{"v":0.32760286199999994,"d":"0.33"}]
["48337","Montague","TX",{"v":0.17746006,"d":"0.18"},{"v":0.9113350263284539,"d":"0.91"},{"v":0.9113350263284536,"d":"0.91"},{"v":0.35313514999999995,"d":"0.35"}]
["48339","Montgomery","TX",{"v":0.123748493,"d":"0.12"},{"v":0.8589797155133244,"d":"0.86"},{"v":0.8589797155133244,"d":"0.86"},{"v":0.38202391399999996,"d":"0.38"}]
["48341","Moore","TX",{"v":0.164697827,"d":"0.16"},{"v":0.9242828396027143,"d":"0.92"},{"v":0.9242828396027143,"d":"0.92"},{"v":0.29364885299999993,"d":"0.29"}]
["48343","Morris","TX",{"v":0.173837882,"d":"0.17"},{"v":0.8666837922359941,"d":"0.87"},{"v":0.8666837922359942,"d":"0.87"},{"v":0.4312527675,"d":"0.43"}]
["48345","Motley","TX",{"v":0.20309547099999997,"d":"0.20"},{"v":0.9737184894209864,"d":"0.97"},{"v":0.9737184894209864,"d":"0.97"},{"v":0.35431969500000005,"d":"0.35"}]
["48347","Nacogdoches","TX",{"v":0.150171328,"d":"0.15"},{"v":0.9116239918248337,"d":"0.91"},{"v":0.9116239918248337,"d":"0.91"},{"v":0.42430263549999997,"d":"0.42"}]
["48349","Navarro","TX",{"v":0.17363803399999997,"d":"0.17"},{"v":0.9114253116973668,"d":"0.91"},{"v":0.9114253116973668,"d":"0.91"},{"v":0.3396747965,"d":"0.34"}]
["48351","Newton","TX",{"v":0.17167499799999997,"d":"0.17"},{"v":0.9539431885592008,"d":"0.95"},{"v":0.9539431885592006,"d":"0.95"},{"v":0.5070627055,"d":"0.51"}]
["48353","Nolan","TX",{"v":0.161227879,"d":"0.16"},{"v":0.8979108309331506,"d":"0.90"},{"v":0.8979108309331506,"d":"0.90"},{"v":0.34306445299999994,"d":"0.34"}]
["48355","Nueces","TX",{"v":0.14467420599999997,"d":"0.14"},{"v":0.8361056247722501,"d":"0.84"},{"v":0.8361056247722499,"d":"0.84"},{"v":0.255309324,"d":"0.26"}]
["48357","Ochiltree","TX",{"v":0.161339886,"d":"0.16"},{"v":0.9026744108148471,"d":"0.90"},{"v":0.902674410814847,"d":"0.90"},{"v":0.2912868965,"d":"0.29"}]
["48359","Oldham","TX",{"v":0.20181969699999996,"d":"0.20"},{"v":0.906408716001304,"d":"0.91"},{"v":0.9064087160013042,"d":"0.91"},{"v":0.35281468899999996,"d":"0.35"}]
["48361","Orange","TX",{"v":0.14760424700000002,"d":"0.15"},{"v":0.8493569415313071,"d":"0.85"},{"v":0.8493569415313071,"d":"0.85"},{"v":0.36080576449999996,"d":"0.36"}]
["48363","Palo Pinto","TX",{"v":0.167449417,"d":"0.17"},{"v":0.9155806636094554,"d":"0.92"},{"v":0.9155806636094553,"d":"0.92"},{"v":0.37149695899999996,"d":"0.37"}]
["48365","Panola","TX",{"v":0.165961346,"d":"0.17"},{"v":0.9356151274440462,"d":"0.94"},{"v":0.9356151274440462,"d":"0.94"},{"v":0.43666853400000005,"d":"0.44"}]
["48367","Parker","TX",{"v":0.168708199,"d":"0.17"},{"v":0.9471782363789563,"d":"0.95"},{"v":0.9471782363789563,"d":"0.95"},{"v":0.34673230600000005,"d":"0.35"}]
["48369","Parmer","TX",{"v":0.183765374,"d":"0.18"},{"v":0.9301702874386574,"d":"0.93"},{"v":0.9301702874386574,"d":"0.93"},{"v":0.32441361649999995,"d":"0.32"}]
["48371","Pecos","TX",{"v":0.17027387,"d":"0.17"},{"v":0.9036996555382131,"d":"0.90"},{"v":0.9036996555382131,"d":"0.90"},{"v":0.31372394800000003,"d":"0.31"}]
["48373","Polk","TX",{"v":0.161962512,"d":"0.16"},{"v":0.9529274450816494,"d":"0.95"},{"v":0.9529274450816494,"d":"0.95"},{"v":0.47488505750000004,"d":"0.47"}]
["48375","Potter","TX",{"v":0.149405425,"d":"0.15"},{"v":0.8969789624394672,"d":"0.90"},{"v":0.896978962439467,"d":"0.90"},{"v":0.283653827,"d":"0.28"}]
["48377","Presidio","TX",{"v":0.182028212,"d":"0.18"},{"v":0.9224130743271213,"d":"0.92"},{"v":0.9224130743271213,"d":"0.92"},{"v":0.31483814450000003,"d":"0.31"}]
["48379","Rains","TX",{"v":0.19036395899999997,"d":"0.19"},{"v":0.9522181887112678,"d":"0.95"},{"v":0.9522181887112678,"d":"0.95"},{"v":0.3773944715,"d":"0.38"}]
["48381","Randall","TX",{"v":0.152126939,"d":"0.15"},{"v":0.9177400039882135,"d":"0.92"},{"v":0.9177400039882135,"d":"0.92"},{"v":0.284759697,"d":"0.28"}]
["48383","Reagan","TX",{"v":0.166318047,"d":"0.17"},{"v":0.885178055191186,"d":"0.89"},{"v":0.885178055191186,"d":"0.89"},{"v":0.2881268435,"d":"0.29"}]
["48385","Real","TX",{"v":0.18613611600000002,"d":"0.19"},{"v":0.9695022900750495,"d":"0.97"},{"v":0.9695022900750495,"d":"0.97"},{"v":0.42247096049999994,"d":"0.42"}]
["48387","Red River","TX",{"v":0.17751851100000002,"d":"0.18"},{"v":0.906062319316332,"d":"0.91"},{"v":0.906062319316332,"d":"0.91"},{"v":0.4047338985,"d":"0.40"}]
["48389","Reeves","TX",{"v":0.170354889,"d":"0.17"},{"v":0.8407801279198438,"d":"0.84"},{"v":0.8407801279198438,"d":"0.84"},{"v":0.289142741,"d":"0.29"}]
["48391","Refugio","TX",{"v":0.186351199,"d":"0.19"},{"v":0.8537191364338369,"d":"0.85"},{"v":0.8537191364338371,"d":"0.85"},{"v":0.3357725905,"d":"0.34"}]
["48393","Roberts","TX",{"v":0.20274393500000001,"d":"0.20"},{"v":0.9500766563881461,"d":"0.95"},{"v":0.9500766563881459,"d":"0.95"},{"v":0.35016033550000003,"d":"0.35"}]
["48395","Robertson","TX",{"v":0.181613957,"d":"0.18"},{"v":0.9104998101930316,"d":"0.91"},{"v":0.9104998101930317,"d":"0.91"},{"v":0.3785539200000001,"d":"0.38"}]
["48397","Rockwall","TX",{"v":0.12990107500000003,"d":"0.13"},{"v":0.8326681444603449,"d":"0.83"},{"v":0.8326681444603448,"d":"0.83"},{"v":0.2830986490000001,"d":"0.28"}]
["48399","Runnels","TX",{"v":0.173407355,"d":"0.17"},{"v":0.8944964988959864,"d":"0.89"},{"v":0.8944964988959864,"d":"0.89"},{"v":0.326871385,"d":"0.33"}]
["48401","Rusk","TX",{"v":0.167874049,"d":"0.17"},{"v":0.911341433314835,"d":"0.91"},{"v":0.9113414333148349,"d":"0.91"},{"v":0.42076136149999993,"d":"0.42"}]
["48403","Sabine","TX",{"v":0.17816369600000004,"d":"0.18"},{"v":0.9732595236402186,"d":"0.97"},{"v":0.9732595236402185,"d":"0.97"},{"v":0.45332152600000003,"d":"0.45"}]
["48405","San Augustine","TX",{"v":0.18035639299999998,"d":"0.18"},{"v":0.9421371645707484,"d":"0.94"},{"v":0.9421371645707484,"d":"0.94"},{"v":0.46199037550000005,"d":"0.46"}]
["48407","San Jacinto","TX",{"v":0.176918319,"d":"0.18"},{"v":0.9733276992336559,"d":"0.97"},{"v":0.9733276992336559,"d":"0.97"},{"v":0.46274423650000013,"d":"0.46"}]
["48409","San Patricio","TX",{"v":0.168427788,"d":"0.17"},{"v":0.8527206005055981,"d":"0.85"},{"v":0.8527206005055981,"d":"0.85"},{"v":0.2813981105,"d":"0.28"}]
["48411","San Saba","TX",{"v":0.17619218099999998,"d":"0.18"},{"v":0.9033718059417098,"d":"0.90"},{"v":0.9033718059417098,"d":"0.90"},{"v":0.3664193155,"d":"0.37"}]
["48413","Schleicher","TX",{"v":0.20084202,"d":"0.20"},{"v":0.906966272392353,"d":"0.91"},{"v":0.9069662723923531,"d":"0.91"},{"v":0.360765747,"d":"0.36"}]
["48415","Scurry","TX",{"v":0.16904244300000001,"d":"0.17"},{"v":0.9068098506415507,"d":"0.91"},{"v":0.9068098506415507,"d":"0.91"},{"v":0.310597519,"d":"0.31"}]
["48417","Shackelford","TX",{"v":0.203173844,"d":"0.20"},{"v":0.9117075118155297,"d":"0.91"},{"v":0.9117075118155297,"d":"0.91"},{"v":0.34625579,"d":"0.35"}]
["48419","Shelby","TX",{"v":0.168559493,"d":"0.17"},{"v":0.9321994503776151,"d":"0.93"},{"v":0.9321994503776153,"d":"0.93"},{"v":0.458128571,"d":"0.46"}]
["48421","Sherman","TX",{"v":0.203796098,"d":"0.20"},{"v":0.9225620833812868,"d":"0.92"},{"v":0.9225620833812868,"d":"0.92"},{"v":0.3425413785,"d":"0.34"}]
["48423","Smith","TX",{"v":0.142076455,"d":"0.14"},{"v":0.8812472440453331,"d":"0.88"},{"v":0.8812472440453332,"d":"0.88"},{"v":0.38181988250000004,"d":"0.38"}]
["48425","Somervell","TX",{"v":0.188918602,"d":"0.19"},{"v":0.9575677083112716,"d":"0.96"},{"v":0.9575677083112714,"d":"0.96"},{"v":0.3938017015000001,"d":"0.39"}]
["48427","Starr","TX",{"v":0.173035569,"d":"0.17"},{"v":0.8676470283592849,"d":"0.87"},{"v":0.8676470283592848,"d":"0.87"},{"v":0.29057439100000004,"d":"0.29"}]
["48429","Stephens","TX",{"v":0.166748772,"d":"0.17"},{"v":0.9155505057713369,"d":"0.92"},{"v":0.9155505057713368,"d":"0.92"},{"v":0.3377617845,"d":"0.34"}]
["48431","Sterling","TX",{"v":0.20497810500000002,"d":"0.20"},{"v":0.9204461790145986,"d":"0.92"},{"v":0.9204461790145986,"d":"0.92"},{"v":0.34771280899999996,"d":"0.35"}]
["48433","Stonewall","TX",{"v":0.197675662,"d":"0.20"},{"v":0.9711559438205918,"d":"0.97"},{"v":0.9711559438205917,"d":"0.97"},{"v":0.3719458195,"d":"0.37"}]
["48435","Sutton","TX",{"v":0.16233639900000002,"d":"0.16"},{"v":0.8998829587911337,"d":"0.90"},{"v":0.8998829587911338,"d":"0.90"},{"v":0.31898154950000007,"d":"0.32"}]
["48437","Swisher","TX",{"v":0.17594186599999997,"d":"0.18"},{"v":0.9028508286605733,"d":"0.90"},{"v":0.9028508286605735,"d":"0.90"},{"v":0.3131793135,"d":"0.31"}]
["48439","Tarrant","TX",{"v":0.073246447,"d":"0.07"},{"v":0.042586209612798846,"d":"0.04"},{"v":0.042586209612798846,"d":"0.04"},{"v":0.237244151,"d":"0.24"}]
["48441","Taylor","TX",{"v":0.14779819599999997,"d":"0.15"},{"v":0.9016109882900378,"d":"0.90"},{"v":0.9016109882900378,"d":"0.90"},{"v":0.32338511499999995,"d":"0.32"}]
["48443","Terrell","TX",{"v":0.205184046,"d":"0.21"},{"v":0.9275247148907685,"d":"0.93"},{"v":0.9275247148907685,"d":"0.93"},{"v":0.35140289750000003,"d":"0.35"}]
["48445","Terry","TX",{"v":0.166887682,"d":"0.17"},{"v":0.9117293253467186,"d":"0.91"},{"v":0.9117293253467187,"d":"0.91"},{"v":0.30266021249999997,"d":"0.30"}]
["48447","Throckmorton","TX",{"v":0.205561744,"d":"0.21"},{"v":0.9052827648410032,"d":"0.91"},{"v":0.9052827648410033,"d":"0.91"},{"v":0.346943623,"d":"0.35"}]
["48449","Titus","TX",{"v":0.164156423,"d":"0.16"},{"v":0.9142621378003248,"d":"0.91"},{"v":0.9142621378003248,"d":"0.91"},{"v":0.37538950600000004,"d":"0.38"}]
["48451","Tom Green","TX",{"v":0.15623046099999996,"d":"0.16"},{"v":0.893057513313191,"d":"0.89"},{"v":0.8930575133131909,"d":"0.89"},{"v":0.2994901155,"d":"0.30"}]
["48453","Travis","TX",{"v":0.09883589999999999,"d":"0.10"},{"v":0.5135857183155208,"d":"0.51"},{"v":0.5135857183155209,"d":"0.51"},{"v":0.2885559275,"d":"0.29"}]
["48455","Trinity","TX",{"v":0.165675214,"d":"0.17"},{"v":0.965976551416222,"d":"0.97"},{"v":0.965976551416222,"d":"0.97"},{"v":0.46002040099999997,"d":"0.46"}]
["48457","Tyler","TX",{"v":0.16609835,"d":"0.17"},{"v":0.9659588079385312,"d":"0.97"},{"v":0.9659588079385312,"d":"0.97"},{"v":0.4972489835,"d":"0.50"}]
["48459","Upshur","TX",{"v":0.17085470900000002,"d":"0.17"},{"v":0.9263611942342621,"d":"0.93"},{"v":0.9263611942342623,"d":"0.93"},{"v":0.4259798074999999,"d":"0.43"}]
["48461","Upton","TX",{"v":0.21011904199999998,"d":"0.21"},{"v":0.8944248751250996,"d":"0.89"},{"v":0.8944248751250996,"d":"0.89"},{"v":0.334702056,"d":"0.33"}]
["48463","Uvalde","TX",{"v":0.16513132999999997,"d":"0.17"},{"v":0.9178163688533632,"d":"0.92"},{"v":0.9178163688533632,"d":"0.92"},{"v":0.33418008849999997,"d":"0.33"}]
["48465","Val Verde","TX",{"v":0.16402270699999996,"d":"0.16"},{"v":0.8985950790349372,"d":"0.90"},{"v":0.8985950790349372,"d":"0.90"},{"v":0.29839186599999995,"d":"0.30"}]
["48467","Van Zandt","TX",{"v":0.179703731,"d":"0.18"},{"v":0.9278273884076851,"d":"0.93"},{"v":0.9278273884076851,"d":"0.93"},{"v":0.37125802499999994,"d":"0.37"}]
["48469","Victoria","TX",{"v":0.16253373299999999,"d":"0.16"},{"v":0.8497630736325339,"d":"0.85"},{"v":0.8497630736325339,"d":"0.85"},{"v":0.31456744500000006,"d":"0.31"}]
["48471","Walker","TX",{"v":0.14670375,"d":"0.15"},{"v":0.9282259252318779,"d":"0.93"},{"v":0.9282259252318779,"d":"0.93"},{"v":0.416623317,"d":"0.42"}]
["48473","Waller","TX",{"v":0.17735974699999998,"d":"0.18"},{"v":0.9290502650885297,"d":"0.93"},{"v":0.9290502650885297,"d":"0.93"},{"v":0.3556806940000001,"d":"0.36"}]
["48475","Ward","TX",{"v":0.172375542,"d":"0.17"},{"v":0.8687526134432718,"d":"0.87"},{"v":0.8687526134432718,"d":"0.87"},{"v":0.2958727475,"d":"0.30"}]
["48477","Washington","TX",{"v":0.17612885300000003,"d":"0.18"},{"v":0.8715607558501748,"d":"0.87"},{"v":0.8715607558501746,"d":"0.87"},{"v":0.34044440449999996,"d":"0.34"}]
["48479","Webb","TX",{"v":0.159506649,"d":"0.16"},{"v":0.8632544165074713,"d":"0.86"},{"v":0.8632544165074713,"d":"0.86"},{"v":0.268462888,"d":"0.27"}]
["48481","Wharton","TX",{"v":0.177992051,"d":"0.18"},{"v":0.8571825689465462,"d":"0.86"},{"v":0.8571825689465462,"d":"0.86"},{"v":0.3218770904999999,"d":"0.32"}]
["48483","Wheeler","TX",{"v":0.20460320699999998,"d":"0.20"},{"v":0.8966035380438643,"d":"0.90"},{"v":0.8966035380438644,"d":"0.90"},{"v":0.347152576,"d":"0.35"}]
["48485","Wichita","TX",{"v":0.150198427,"d":"0.15"},{"v":0.888074581135637,"d":"0.89"},{"v":0.888074581135637,"d":"0.89"},{"v":0.27797598800000006,"d":"0.28"}]
["48487","Wilbarger","TX",{"v":0.16596979499999998,"d":"0.17"},{"v":0.870741045215961,"d":"0.87"},{"v":0.8707410452159611,"d":"0.87"},{"v":0.301444306,"d":"0.30"}]
["48489","Willacy","TX",{"v":0.183850952,"d":"0.18"},{"v":0.8416790446808574,"d":"0.84"},{"v":0.8416790446808574,"d":"0.84"},{"v":0.296826691,"d":"0.30"}]
["48491","Williamson","TX",{"v":0.13435495399999997,"d":"0.13"},{"v":0.855847944314504,"d":"0.86"},{"v":0.8558479443145041,"d":"0.86"},{"v":0.29679743550000004,"d":"0.30"}]
["48493","Wilson","TX",{"v":0.192926427,"d":"0.19"},{"v":0.906307375318012,"d":"0.91"},{"v":0.9063073753180118,"d":"0.91"},{"v":0.35141491150000004,"d":"0.35"}]
["48495","Winkler","TX",{"v":0.16839724200000003,"d":"0.17"},{"v":0.8459641444902296,"d":"0.85"},{"v":0.8459641444902296,"d":"0.85"},{"v":0.28591889099999995,"d":"0.29"}]
["48497","Wise","TX",{"v":0.18074414199999997,"d":"0.18"},{"v":0.9588188372042412,"d":"0.96"},{"v":0.9588188372042412,"d":"0.96"},{"v":0.3538388895,"d":"0.35"}]
["48499","Wood","TX",{"v":0.173180231,"d":"0.17"},{"v":0.9304104344018552,"d":"0.93"},{"v":0.9304104344018553,"d":"0.93"},{"v":0.41138130450000004,"d":"0.41"}]
["48501","Yoakum","TX",{"v":0.171583596,"d":"0.17"},{"v":0.9424084692343564,"d":"0.94"},{"v":0.9424084692343563,"d":"0.94"},{"v":0.31309330399999996,"d":"0.31"}]
["48503","Young","TX",{"v":0.168410163,"d":"0.17"},{"v":0.8995629460798578,"d":"0.90"},{"v":0.8995629460798578,"d":"0.90"},{"v":0.3272425395,"d":"0.33"}]
["48505","Zapata","TX",{"v":0.174675797,"d":"0.17"},{"v":0.8971668158413525,"d":"0.90"},{"v":0.8971668158413525,"d":"0.90"},{"v":0.29053264800000006,"d":"0.29"}]
["48507","Zavala","TX",{"v":0.178140746,"d":"0.18"},{"v":0.8569347409554158,"d":"0.86"},{"v":0.8569347409554158,"d":"0.86"},{"v":0.30992110700000003,"d":"0.31"}]
["49001","Beaver","UT",{"v":0.10809661,"d":"0.11"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.238913916,"d":"0.24"}]
["49003","Box Elder","UT",{"v":0.106328074,"d":"0.11"},{"v":0.6425833757193896,"d":"0.64"},{"v":0.6425833757193896,"d":"0.64"},{"v":0.21118393849999995,"d":"0.21"}]
["49005","Cache","UT",{"v":0.096303747,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.22094791199999997,"d":"0.22"}]
["49007","Carbon","UT",{"v":0.10262777099999999,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.22827585399999994,"d":"0.23"}]
["49009","Daggett","UT",{"v":0.110180648,"d":"0.11"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.2874065515,"d":"0.29"}]
["49011","Davis","UT",{"v":0.06681833100000001,"d":"0.07"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.179229379,"d":"0.18"}]
["49013","Duchesne","UT",{"v":0.11029585599999998,"d":"0.11"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.25383471599999996,"d":"0.25"}]
["49015","Emery","UT",{"v":0.11883861200000001,"d":"0.12"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.23268638049999993,"d":"0.23"}]
["49017","Garfield","UT",{"v":0.119902463,"d":"0.12"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.259416001,"d":"0.26"}]
["49019","Grand","UT",{"v":0.101612636,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.21779130700000007,"d":"0.22"}]
["49021","Iron","UT",{"v":0.09773466,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.22229674200000002,"d":"0.22"}]
["49023","Juab","UT",{"v":0.108932732,"d":"0.11"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.22228614400000002,"d":"0.22"}]
["49025","Kane","UT",{"v":0.109068936,"d":"0.11"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.23558687849999996,"d":"0.24"}]
["49027","Millard","UT",{"v":0.11622661100000001,"d":"0.12"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.23308490849999997,"d":"0.23"}]
["49029","Morgan","UT",{"v":0.103663181,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.2727653355,"d":"0.27"}]
["49031","Piute","UT",{"v":0.11785852000000001,"d":"0.12"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.2676305005,"d":"0.27"}]
["49033","Rich","UT",{"v":0.118078042,"d":"0.12"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.26479623900000004,"d":"0.26"}]
["49035","Salt Lake","UT",{"v":0.05674297100000002,"d":"0.06"},{"v":0.34057512367782844,"d":"0.34"},{"v":0.34057512367782844,"d":"0.34"},{"v":0.18219874900000002,"d":"0.18"}]
["49037","San Juan","UT",{"v":0.117461381,"d":"0.12"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.23699911699999998,"d":"0.24"}]
["49039","Sanpete","UT",{"v":0.10118272100000002,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.245398213,"d":"0.25"}]
["49041","Sevier","UT",{"v":0.107250135,"d":"0.11"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.2561868705,"d":"0.26"}]
["49043","Summit","UT",{"v":0.09257777199999999,"d":"0.09"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.2610500295,"d":"0.26"}]
["49045","Tooele","UT",{"v":0.10278664800000001,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.20350348199999999,"d":"0.20"}]
["49047","Uintah","UT",{"v":0.105693701,"d":"0.11"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.23393557099999995,"d":"0.23"}]
["49049","Utah","UT",{"v":0.086210564,"d":"0.09"},{"v":0.6492107964544159,"d":"0.65"},{"v":0.6492107964544159,"d":"0.65"},{"v":0.21076308,"d":"0.21"}]
["49051","Wasatch","UT",{"v":0.092250028,"d":"0.09"},{"v":0.7463449948393819,"d":"0.75"},{"v":0.7463449948393819,"d":"0.75"},{"v":0.25793347299999997,"d":"0.26"}]
["49053","Washington","UT",{"v":0.104019742,"d":"0.10"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.1987780425,"d":"0.20"}]
["49055","Wayne","UT",{"v":0.126347204,"d":"0.13"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.2400570715,"d":"0.24"}]
["49057","Weber","UT",{"v":0.079033878,"d":"0.08"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.2139013545,"d":"0.21"}]
["50001","Addison","VT",{"v":0.7223465023074824,"d":"0.72"},{"v":5.872589137735086,"d":"5.87"},{"v":5.872589137735085,"d":"5.87"},{"v":2.328585201652495,"d":"2.33"}]
["50003","Bennington","VT",{"v":0.6497887273881637,"d":"0.65"},{"v":5.97070000060607,"d":"5.97"},{"v":5.97070000060607,"d":"5.97"},{"v":2.676854925297747,"d":"2.68"}]
["50005","Caledonia","VT",{"v":0.6637542292919774,"d":"0.66"},{"v":6.18794779139361,"d":"6.19"},{"v":6.18794779139361,"d":"6.19"},{"v":2.549624351436727,"d":"2.55"}]
["50007","Chittenden","VT",{"v":0.5804027525126736,"d":"0.58"},{"v":5.369971978585269,"d":"5.37"},{"v":5.369971978585269,"d":"5.37"},{"v":2.075313894207269,"d":"2.08"}]
["50009","Essex","VT",{"v":0.7081557539531658,"d":"0.71"},{"v":6.313481195304431,"d":"6.31"},{"v":6.313481195304431,"d":"6.31"},{"v":2.722747031505327,"d":"2.72"}]
["50011","Franklin","VT",{"v":0.6893805771476893,"d":"0.69"},{"v":5.724970966609709,"d":"5.72"},{"v":5.724970966609709,"d":"5.72"},{"v":2.2694816731433463,"d":"2.27"}]
["50013","Grand Isle","VT",{"v":0.8219268200094654,"d":"0.82"},{"v":5.6664869191886975,"d":"5.67"},{"v":5.6664869191886975,"d":"5.67"},{"v":1.939280259313013,"d":"1.94"}]
["50015","Lamoille","VT",{"v":0.7131201898829,"d":"0.71"},{"v":6.164746623138796,"d":"6.16"},{"v":6.164746623138796,"d":"6.16"},{"v":2.7341012742874504,"d":"2.73"}]
["50017","Orange","VT",{"v":0.7053889552907281,"d":"0.71"},{"v":6.248626767071464,"d":"6.25"},{"v":6.248626767071464,"d":"6.25"},{"v":2.6492578524922403,"d":"2.65"}]
["50019","Orleans","VT",{"v":0.7005401059743711,"d":"0.70"},{"v":6.158417757146905,"d":"6.16"},{"v":6.158417757146904,"d":"6.16"},{"v":2.4903507608012023,"d":"2.49"}]
["50021","Rutland","VT",{"v":0.6396312827058506,"d":"0.64"},{"v":5.893481486833162,"d":"5.89"},{"v":5.893481486833162,"d":"5.89"},{"v":2.515696666086637,"d":"2.52"}]
["50023","Washington","VT",{"v":0.6181112246216535,"d":"0.62"},{"v":6.150844954433153,"d":"6.15"},{"v":6.150844954433153,"d":"6.15"},{"v":2.5297184359055667,"d":"2.53"}]
["50025","Windham","VT",{"v":0.6596461358588643,"d":"0.66"},{"v":6.037816301547804,"d":"6.04"},{"v":6.037816301547803,"d":"6.04"},{"v":2.6506201890879555,"d":"2.65"}]
["50027","Windsor","VT",{"v":0.66657550775674,"d":"0.67"},{"v":5.945247228987526,"d":"5.95"},{"v":5.945247228987528,"d":"5.95"},{"v":2.625900953800334,"d":"2.63"}]
["51001","Accomack","VA",{"v":0.388196532,"d":"0.39"},{"v":2.0758360065686907,"d":"2.08"},{"v":2.0758360065686907,"d":"2.08"},{"v":0.7471968155000001,"d":"0.75"}]
["51003","Albemarle","VA",{"v":0.288702105,"d":"0.29"},{"v":2.165561815961992,"d":"2.17"},{"v":2.165561815961992,"d":"2.17"},{"v":0.959567207,"d":"0.96"}]
["51005","Alleghany","VA",{"v":0.276489268,"d":"0.28"},{"v":2.2064579993351003,"d":"2.21"},{"v":2.2064579993351003,"d":"2.21"},{"v":1.122422774,"d":"1.12"}]
["51007","Amelia","VA",{"v":0.343222158,"d":"0.34"},{"v":2.196878641338961,"d":"2.20"},{"v":2.1968786413389605,"d":"2.20"},{"v":0.9997587535000001,"d":"1.00"}]
["51009","Amherst","VA",{"v":0.301942793,"d":"0.30"},{"v":2.156050874878728,"d":"2.16"},{"v":2.156050874878728,"d":"2.16"},{"v":1.045319553,"d":"1.05"}]
["51011","Appomattox","VA",{"v":0.338138218,"d":"0.34"},{"v":2.1887052624004597,"d":"2.19"},{"v":2.1887052624004597,"d":"2.19"},{"v":0.9982133375000001,"d":"1.00"}]
["51013","Arlington","VA",{"v":0.014060444999999998,"d":"0.01"},{"v":1.89880524348764e-15,"d":"0.00"},{"v":1.89880524348764e-15,"d":"0.00"},{"v":0.3707130215,"d":"0.37"}]
["51015","Augusta","VA",{"v":0.307976748,"d":"0.31"},{"v":2.2167058907580475,"d":"2.22"},{"v":2.216705890758048,"d":"2.22"},{"v":0.9611244475000001,"d":"0.96"}]
["51017","Bath","VA",{"v":0.32075669399999995,"d":"0.32"},{"v":2.272729582127798,"d":"2.27"},{"v":2.272729582127798,"d":"2.27"},{"v":1.191134941,"d":"1.19"}]
["51019","Bedford","VA",{"v":0.321321203,"d":"0.32"},{"v":2.17418034794139,"d":"2.17"},{"v":2.17418034794139,"d":"2.17"},{"v":0.953581339,"d":"0.95"}]
["51021","Bland","VA",{"v":0.32691749300000006,"d":"0.33"},{"v":2.3075914087328764,"d":"2.31"},{"v":2.307591408732877,"d":"2.31"},{"v":1.0837050279999998,"d":"1.08"}]
["51023","Botetourt","VA",{"v":0.29903365299999995,"d":"0.30"},{"v":2.1982494549545497,"d":"2.20"},{"v":2.1982494549545497,"d":"2.20"},{"v":1.0423146815,"d":"1.04"}]
["51025","Brunswick","VA",{"v":0.32426104699999997,"d":"0.32"},{"v":2.1861033019973246,"d":"2.19"},{"v":2.1861033019973246,"d":"2.19"},{"v":1.0183269929999998,"d":"1.02"}]
["51027","Buchanan","VA",{"v":0.31416246999999997,"d":"0.31"},{"v":2.3376111821468353,"d":"2.34"},{"v":2.3376111821468353,"d":"2.34"},{"v":1.1252767469999998,"d":"1.13"}]
["51029","Buckingham","VA",{"v":0.332962525,"d":"0.33"},{"v":2.212052694985182,"d":"2.21"},{"v":2.212052694985182,"d":"2.21"},{"v":1.0302862649999998,"d":"1.03"}]
["51031","Campbell","VA",{"v":0.30800304900000003,"d":"0.31"},{"v":2.163972014746101,"d":"2.16"},{"v":2.1639720147461015,"d":"2.16"},{"v":0.9165750585,"d":"0.92"}]
["51033","Caroline","VA",{"v":0.32685403999999996,"d":"0.33"},{"v":2.151763674234858,"d":"2.15"},{"v":2.151763674234858,"d":"2.15"},{"v":0.9948332810000001,"d":"0.99"}]
["51035","Carroll","VA",{"v":0.331222837,"d":"0.33"},{"v":2.2618681550098594,"d":"2.26"},{"v":2.2618681550098594,"d":"2.26"},{"v":1.0029214494999998,"d":"1.00"}]
["51036","Charles City","VA",{"v":0.353629766,"d":"0.35"},{"v":2.1196305179196386,"d":"2.12"},{"v":2.1196305179196386,"d":"2.12"},{"v":0.9451741780000001,"d":"0.95"}]
["51037","Charlotte","VA",{"v":0.3399306670000001,"d":"0.34"},{"v":2.203550701391943,"d":"2.20"},{"v":2.2035507013919435,"d":"2.20"},{"v":1.0080561030000001,"d":"1.01"}]
["51041","Chesterfield","VA",{"v":0.21077927199999996,"d":"0.21"},{"v":1.830442086386182,"d":"1.83"},{"v":1.8304420863861819,"d":"1.83"},{"v":0.813441162,"d":"0.81"}]
["51043","Clarke","VA",{"v":0.327591601,"d":"0.33"},{"v":2.1337136285964946,"d":"2.13"},{"v":2.133713628596494,"d":"2.13"},{"v":0.8507581285000002,"d":"0.85"}]
["51045","Craig","VA",{"v":0.314927557,"d":"0.31"},{"v":2.313930287426732,"d":"2.31"},{"v":2.3139302874267313,"d":"2.31"},{"v":1.138421783,"d":"1.14"}]
["51047","Culpeper","VA",{"v":0.315648649,"d":"0.32"},{"v":2.1178231185675185,"d":"2.12"},{"v":2.1178231185675185,"d":"2.12"},{"v":0.8655116335000002,"d":"0.87"}]
["51049","Cumberland","VA",{"v":0.33549002400000005,"d":"0.34"},{"v":2.14831679822596,"d":"2.15"},{"v":2.14831679822596,"d":"2.15"},{"v":1.0087670760000003,"d":"1.01"}]
["51051","Dickenson","VA",{"v":0.316705103,"d":"0.32"},{"v":2.331210783388716,"d":"2.33"},{"v":2.331210783388716,"d":"2.33"},{"v":1.1032138065000001,"d":"1.10"}]
["51053","Dinwiddie","VA",{"v":0.316133339,"d":"0.32"},{"v":2.1431116344259733,"d":"2.14"},{"v":2.1431116344259733,"d":"2.14"},{"v":0.9756124179999999,"d":"0.98"}]
["51057","Essex","VA",{"v":0.3310506389999999,"d":"0.33"},{"v":2.077607864402679,"d":"2.08"},{"v":2.0776078644026788,"d":"2.08"},{"v":0.9040794979999999,"d":"0.90"}]
["51059","Fairfax","VA",{"v":0.11580826999999999,"d":"0.12"},{"v":0.012778659265358308,"d":"0.01"},{"v":0.012778659265358304,"d":"0.01"},{"v":0.5816008295,"d":"0.58"}]
["51061","Fauquier","VA",{"v":0.318210577,"d":"0.32"},{"v":2.147133773991342,"d":"2.15"},{"v":2.147133773991342,"d":"2.15"},{"v":0.8724102294999999,"d":"0.87"}]
["51063","Floyd","VA",{"v":0.333929529,"d":"0.33"},{"v":2.261505448069992,"d":"2.26"},{"v":2.261505448069992,"d":"2.26"},{"v":1.027826677,"d":"1.03"}]
["51065","Fluvanna","VA",{"v":0.302991621,"d":"0.30"},{"v":2.129482171099415,"d":"2.13"},{"v":2.129482171099415,"d":"2.13"},{"v":0.979639882,"d":"0.98"}]
["51067","Franklin","VA",{"v":0.329563954,"d":"0.33"},{"v":2.1697234868964665,"d":"2.17"},{"v":2.1697234868964665,"d":"2.17"},{"v":0.9562305665,"d":"0.96"}]
["51069","Frederick","VA",{"v":0.291670439,"d":"0.29"},{"v":2.152651536999602,"d":"2.15"},{"v":2.152651536999602,"d":"2.15"},{"v":0.914546849,"d":"0.91"}]
["51071","Giles","VA",{"v":0.298125339,"d":"0.30"},{"v":2.2282100589322007,"d":"2.23"},{"v":2.2282100589322007,"d":"2.23"},{"v":1.048789269,"d":"1.05"}]
["51073","Gloucester","VA",{"v":0.321368908,"d":"0.32"},{"v":2.071547771714056,"d":"2.07"},{"v":2.071547771714056,"d":"2.07"},{"v":0.8400950700000002,"d":"0.84"}]
["51075","Goochland","VA",{"v":0.33813969,"d":"0.34"},{"v":2.1228130474715408,"d":"2.12"},{"v":2.1228130474715408,"d":"2.12"},{"v":1.0068662295000002,"d":"1.01"}]
["51077","Grayson","VA",{"v":0.334441726,"d":"0.33"},{"v":2.273888229373853,"d":"2.27"},{"v":2.273888229373853,"d":"2.27"},{"v":1.0323516085000002,"d":"1.03"}]
["51079","Greene","VA",{"v":0.287830375,"d":"0.29"},{"v":2.193404576671018,"d":"2.19"},{"v":2.193404576671018,"d":"2.19"},{"v":0.9824584394999999,"d":"0.98"}]
["51081","Greensville","VA",{"v":0.329481288,"d":"0.33"},{"v":2.14911856801523,"d":"2.15"},{"v":2.1491185680152296,"d":"2.15"},{"v":0.9683143950000002,"d":"0.97"}]
["51083","Halifax","VA",{"v":0.320733678,"d":"0.32"},{"v":2.1781189814748663,"d":"2.18"},{"v":2.1781189814748663,"d":"2.18"},{"v":0.9704148965000003,"d":"0.97"}]
["51085","Hanover","VA",{"v":0.281050634,"d":"0.28"},{"v":2.0519804413489884,"d":"2.05"},{"v":2.0519804413489884,"d":"2.05"},{"v":0.8822259714999999,"d":"0.88"}]
["51087","Henrico","VA",{"v":0.18337006499999997,"d":"0.18"},{"v":0.8074539760201108,"d":"0.81"},{"v":0.8074539760201108,"d":"0.81"},{"v":0.6842540490000001,"d":"0.68"}]
["51089","Henry","VA",{"v":0.29379688,"d":"0.29"},{"v":2.168802044792186,"d":"2.17"},{"v":2.168802044792186,"d":"2.17"},{"v":0.9665184489999997,"d":"0.97"}]
["51091","Highland","VA",{"v":0.330212928,"d":"0.33"},{"v":2.285234915046783,"d":"2.29"},{"v":2.285234915046783,"d":"2.29"},{"v":1.116170967,"d":"1.12"}]
["51093","Isle of Wight","VA",{"v":0.322030769,"d":"0.32"},{"v":2.024715005501722,"d":"2.02"},{"v":2.024715005501722,"d":"2.02"},{"v":0.8176244010000001,"d":"0.82"}]
["51095","James City","VA",{"v":0.25794730500000007,"d":"0.26"},{"v":1.886216114773305,"d":"1.89"},{"v":1.886216114773305,"d":"1.89"},{"v":0.732722328,"d":"0.73"}]
["51097","King and Queen","VA",{"v":0.350109313,"d":"0.35"},{"v":2.1233734372349184,"d":"2.12"},{"v":2.1233734372349184,"d":"2.12"},{"v":0.9896724330000003,"d":"0.99"}]
["51099","King George","VA",{"v":0.33490698299999994,"d":"0.33"},{"v":2.0675085180607264,"d":"2.07"},{"v":2.0675085180607264,"d":"2.07"},{"v":0.8465174975000002,"d":"0.85"}]
["51101","King William","VA",{"v":0.334504329,"d":"0.33"},{"v":2.08738067612389,"d":"2.09"},{"v":2.0873806761238907,"d":"2.09"},{"v":0.9496718310000002,"d":"0.95"}]
["51103","Lancaster","VA",{"v":0.370382902,"d":"0.37"},{"v":2.0712968223484287,"d":"2.07"},{"v":2.0712968223484287,"d":"2.07"},{"v":0.8417619515,"d":"0.84"}]
["51105","Lee","VA",{"v":0.32934530999999995,"d":"0.33"},{"v":2.2654194470986804,"d":"2.27"},{"v":2.2654194470986804,"d":"2.27"},{"v":1.0364429439999998,"d":"1.04"}]
["51107","Loudoun","VA",{"v":0.260131967,"d":"0.26"},{"v":2.0007779021494514,"d":"2.00"},{"v":2.0007779021494514,"d":"2.00"},{"v":0.6930616455000002,"d":"0.69"}]
["51109","Louisa","VA",{"v":0.341399496,"d":"0.34"},{"v":2.1567596066469163,"d":"2.16"},{"v":2.1567596066469163,"d":"2.16"},{"v":0.9984926604999999,"d":"1.00"}]
["51111","Lunenburg","VA",{"v":0.33877485300000004,"d":"0.34"},{"v":2.1849944738740326,"d":"2.18"},{"v":2.1849944738740326,"d":"2.18"},{"v":1.0131253654999999,"d":"1.01"}]
["51113","Madison","VA",{"v":0.343434423,"d":"0.34"},{"v":2.1898933668496348,"d":"2.19"},{"v":2.1898933668496348,"d":"2.19"},{"v":0.9987907365,"d":"1.00"}]
["51115","Mathews","VA",{"v":0.38190866199999995,"d":"0.38"},{"v":2.0401750494584983,"d":"2.04"},{"v":2.0401750494584983,"d":"2.04"},{"v":0.7501759960000002,"d":"0.75"}]
["51117","Mecklenburg","VA",{"v":0.3253354909999999,"d":"0.33"},{"v":2.1507829224871835,"d":"2.15"},{"v":2.150782922487184,"d":"2.15"},{"v":0.9286966415000001,"d":"0.93"}]
["51119","Middlesex","VA",{"v":0.366768598,"d":"0.37"},{"v":2.0761829997328167,"d":"2.08"},{"v":2.0761829997328167,"d":"2.08"},{"v":0.85378789,"d":"0.85"}]
["51121","Montgomery","VA",{"v":0.256441405,"d":"0.26"},{"v":2.179274150971885,"d":"2.18"},{"v":2.179274150971885,"d":"2.18"},{"v":0.910058282,"d":"0.91"}]
["51125","Nelson","VA",{"v":0.333935784,"d":"0.33"},{"v":2.2111452329853427,"d":"2.21"},{"v":2.211145232985343,"d":"2.21"},{"v":1.103150191,"d":"1.10"}]
["51127","New Kent","VA",{"v":0.35047613899999996,"d":"0.35"},{"v":2.0811455572035014,"d":"2.08"},{"v":2.0811455572035014,"d":"2.08"},{"v":0.9574196225000001,"d":"0.96"}]
["51131","Northampton","VA",{"v":0.39750020899999994,"d":"0.40"},{"v":2.041304167828801,"d":"2.04"},{"v":2.041304167828801,"d":"2.04"},{"v":0.7173151735,"d":"0.72"}]
["51133","Northumberland","VA",{"v":0.379853144,"d":"0.38"},{"v":2.0504430700823195,"d":"2.05"},{"v":2.0504430700823195,"d":"2.05"},{"v":0.7852605785,"d":"0.79"}]
["51135","Nottoway","VA",{"v":0.307133091,"d":"0.31"},{"v":2.1464125228723256,"d":"2.15"},{"v":2.1464125228723256,"d":"2.15"},{"v":0.9527505755000002,"d":"0.95"}]
["51137","Orange","VA",{"v":0.304646362,"d":"0.30"},{"v":2.1969130230875096,"d":"2.20"},{"v":2.196913023087509,"d":"2.20"},{"v":0.9088921095000001,"d":"0.91"}]
["51139","Page","VA",{"v":0.315019324,"d":"0.32"},{"v":2.216106655913834,"d":"2.22"},{"v":2.2161066559138334,"d":"2.22"},{"v":1.006225592,"d":"1.01"}]
["51141","Patrick","VA",{"v":0.330708945,"d":"0.33"},{"v":2.224955327596265,"d":"2.22"},{"v":2.224955327596265,"d":"2.22"},{"v":1.0614236315,"d":"1.06"}]
["51143","Pittsylvania","VA",{"v":0.330053222,"d":"0.33"},{"v":2.1757703241585924,"d":"2.18"},{"v":2.1757703241585924,"d":"2.18"},{"v":0.9409700625,"d":"0.94"}]
["51145","Powhatan","VA",{"v":0.33592349900000007,"d":"0.34"},{"v":2.1283108900619214,"d":"2.13"},{"v":2.128310890061921,"d":"2.13"},{"v":1.017351822,"d":"1.02"}]
["51147","Prince Edward","VA",{"v":0.30834871300000005,"d":"0.31"},{"v":2.1425184312841634,"d":"2.14"},{"v":2.1425184312841634,"d":"2.14"},{"v":0.9641973435,"d":"0.96"}]
["51149","Prince George","VA",{"v":0.319900648,"d":"0.32"},{"v":2.0948305678622714,"d":"2.09"},{"v":2.0948305678622714,"d":"2.09"},{"v":0.9308304565000002,"d":"0.93"}]
["51153","Prince William","VA",{"v":0.199103962,"d":"0.20"},{"v":1.4882514295402012,"d":"1.49"},{"v":1.4882514295402012,"d":"1.49"},{"v":0.695383472,"d":"0.70"}]
["51155","Pulaski","VA",{"v":0.293414944,"d":"0.29"},{"v":2.185315804625441,"d":"2.19"},{"v":2.185315804625441,"d":"2.19"},{"v":0.8984899390000002,"d":"0.90"}]
["51157","Rappahannock","VA",{"v":0.338657269,"d":"0.34"},{"v":2.2066602704133897,"d":"2.21"},{"v":2.2066602704133897,"d":"2.21"},{"v":1.040755361,"d":"1.04"}]
["51159","Richmond","VA",{"v":0.3579880959999999,"d":"0.36"},{"v":2.0733751604082773,"d":"2.07"},{"v":2.0733751604082773,"d":"2.07"},{"v":0.888548051,"d":"0.89"}]
["51161","Roanoke","VA",{"v":0.23549523099999997,"d":"0.24"},{"v":2.064914338963454,"d":"2.06"},{"v":2.064914338963454,"d":"2.06"},{"v":0.9529701125000001,"d":"0.95"}]
["51163","Rockbridge","VA",{"v":0.32273205,"d":"0.32"},{"v":2.247767072795575,"d":"2.25"},{"v":2.2477670727955754,"d":"2.25"},{"v":1.0555851274999999,"d":"1.06"}]
["51165","Rockingham","VA",{"v":0.307723315,"d":"0.31"},{"v":2.2513171272625376,"d":"2.25"},{"v":2.2513171272625376,"d":"2.25"},{"v":0.9341740815,"d":"0.93"}]
["51167","Russell","VA",{"v":0.32533803,"d":"0.33"},{"v":2.2783541560372673,"d":"2.28"},{"v":2.2783541560372673,"d":"2.28"},{"v":0.9830498104999998,"d":"0.98"}]
["51169","Scott","VA",{"v":0.315723963,"d":"0.32"},{"v":2.272283564406909,"d":"2.27"},{"v":2.2722835644069086,"d":"2.27"},{"v":0.9965141845,"d":"1.00"}]
["51171","Shenandoah","VA",{"v":0.314425455,"d":"0.31"},{"v":2.189156932976064,"d":"2.19"},{"v":2.1891569329760636,"d":"2.19"},{"v":0.946704112,"d":"0.95"}]
["51173","Smyth","VA",{"v":0.306158959,"d":"0.31"},{"v":2.236025943109199,"d":"2.24"},{"v":2.2360259431091993,"d":"2.24"},{"v":0.995738975,"d":"1.00"}]
["51175","Southampton","VA",{"v":0.352650054,"d":"0.35"},{"v":2.102804410047246,"d":"2.10"},{"v":2.102804410047246,"d":"2.10"},{"v":0.9377589115,"d":"0.94"}]
["51177","Spotsylvania","VA",{"v":0.268650874,"d":"0.27"},{"v":2.044720906836419,"d":"2.04"},{"v":2.044720906836419,"d":"2.04"},{"v":0.891813036,"d":"0.89"}]
["51179","Stafford","VA",{"v":0.256717993,"d":"0.26"},{"v":1.9795655765916562,"d":"1.98"},{"v":1.9795655765916558,"d":"1.98"},{"v":0.8129212874999999,"d":"0.81"}]
["51181","Surry","VA",{"v":0.359890729,"d":"0.36"},{"v":2.1004211294230766,"d":"2.10"},{"v":2.1004211294230766,"d":"2.10"},{"v":0.9076427494999999,"d":"0.91"}]
["51183","Sussex","VA",{"v":0.34170127599999994,"d":"0.34"},{"v":2.1417739334788073,"d":"2.14"},{"v":2.141773933478807,"d":"2.14"},{"v":0.9937682130000001,"d":"0.99"}]
["51185","Tazewell","VA",{"v":0.286411643,"d":"0.29"},{"v":2.2584599853256875,"d":"2.26"},{"v":2.2584599853256875,"d":"2.26"},{"v":0.9613526105,"d":"0.96"}]
["51187","Warren","VA",{"v":0.288155756,"d":"0.29"},{"v":2.196107432669353,"d":"2.20"},{"v":2.1961074326693533,"d":"2.20"},{"v":0.956342093,"d":"0.96"}]
["51191","Washington","VA",{"v":0.311340176,"d":"0.31"},{"v":2.2004557134341614,"d":"2.20"},{"v":2.2004557134341614,"d":"2.20"},{"v":0.931597236,"d":"0.93"}]
["51193","Westmoreland","VA",{"v":0.35469609900000004,"d":"0.35"},{"v":2.06108754051168,"d":"2.06"},{"v":2.0610875405116804,"d":"2.06"},{"v":0.7881858545000001,"d":"0.79"}]
["51195","Wise","VA",{"v":0.2868433630000001,"d":"0.29"},{"v":2.281540580157681,"d":"2.28"},{"v":2.2815405801576816,"d":"2.28"},{"v":0.9881453260000003,"d":"0.99"}]
["51197","Wythe","VA",{"v":0.317429383,"d":"0.32"},{"v":2.2226857118570393,"d":"2.22"},{"v":2.2226857118570393,"d":"2.22"},{"v":0.9189260545,"d":"0.92"}]
["51199","York","VA",{"v":0.255610585,"d":"0.26"},{"v":1.8220078062734824,"d":"1.82"},{"v":1.8220078062734824,"d":"1.82"},{"v":0.638448013,"d":"0.64"}]
["51510","Alexandria City","VA",{"v":0.009970414,"d":"0.01"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.36472925399999995,"d":"0.36"}]
["51520","Bristol City","VA",{"v":0.177514244,"d":"0.18"},{"v":0.6797207766674025,"d":"0.68"},{"v":0.6797207766674025,"d":"0.68"},{"v":0.677950074,"d":"0.68"}]
["51530","Buena Vista City","VA",{"v":0.197378851,"d":"0.20"},{"v":1.5419055727673192,"d":"1.54"},{"v":1.541905572767319,"d":"1.54"},{"v":0.7533101130000001,"d":"0.75"}]
["51540","Charlottesville City","VA",{"v":0.06174969100000001,"d":"0.06"},{"v":4.1873569531352787E-6,"d":"0.00"},{"v":4.1873569531352787E-6,"d":"0.00"},{"v":0.6269763684999999,"d":"0.63"}]
["51550","Chesapeake City","VA",{"v":0.236983261,"d":"0.24"},{"v":1.8406343840648944,"d":"1.84"},{"v":1.8406343840648944,"d":"1.84"},{"v":0.742122782,"d":"0.74"}]
["51570","Colonial Heights City","VA",{"v":0.130306226,"d":"0.13"},{"v":0.022715999570870168,"d":"0.02"},{"v":0.02271599957087017,"d":"0.02"},{"v":0.64021615,"d":"0.64"}]
["51580","Covington City","VA",{"v":0.177490953,"d":"0.18"},{"v":1.29468187690754,"d":"1.29"},{"v":1.2946818769075399,"d":"1.29"},{"v":0.930766241,"d":"0.93"}]
["51590","Danville City","VA",{"v":0.19533228,"d":"0.20"},{"v":1.304611021866697,"d":"1.30"},{"v":1.3046110218666969,"d":"1.30"},{"v":0.7484809465000001,"d":"0.75"}]
["51595","Emporia City","VA",{"v":0.21693914,"d":"0.22"},{"v":1.7829419095177623,"d":"1.78"},{"v":1.7829419095177623,"d":"1.78"},{"v":0.7875746395,"d":"0.79"}]
["51600","Fairfax City","VA",{"v":0.081110407,"d":"0.08"},{"v":3.5712334142768294E-4,"d":"0.00"},{"v":3.5712334142768294E-4,"d":"0.00"},{"v":0.5826812085,"d":"0.58"}]
["51610","Falls Church City","VA",{"v":0.028700685000000004,"d":"0.03"},{"v":8.099756990565169e-10,"d":"0.00"},{"v":8.099756990565169e-10,"d":"0.00"},{"v":0.4540087660000001,"d":"0.45"}]
["51620","Franklin City","VA",{"v":0.20187149300000004,"d":"0.20"},{"v":1.2997425625243475,"d":"1.30"},{"v":1.2997425625243475,"d":"1.30"},{"v":0.6992172449999999,"d":"0.70"}]
["51630","Fredericksburg City","VA",{"v":0.108897808,"d":"0.11"},{"v":0.013214272773322813,"d":"0.01"},{"v":0.013214272773322813,"d":"0.01"},{"v":0.608930138,"d":"0.61"}]
["51640","Galax City","VA",{"v":0.208413793,"d":"0.21"},{"v":1.7371175255440265,"d":"1.74"},{"v":1.7371175255440265,"d":"1.74"},{"v":0.7624317015000001,"d":"0.76"}]
["51650","Hampton City","VA",{"v":0.133608552,"d":"0.13"},{"v":0.008170145755532167,"d":"0.01"},{"v":0.008170145755532168,"d":"0.01"},{"v":0.440068129,"d":"0.44"}]
["51660","Harrisonburg City","VA",{"v":0.11921791499999998,"d":"0.12"},{"v":0.018306469227113858,"d":"0.02"},{"v":0.018306469227113858,"d":"0.02"},{"v":0.512632407,"d":"0.51"}]
["51670","Hopewell City","VA",{"v":0.1414535,"d":"0.14"},{"v":0.03838078133705291,"d":"0.04"},{"v":0.03838078133705291,"d":"0.04"},{"v":0.6037263245000001,"d":"0.60"}]
["51678","Lexington City","VA",{"v":0.102840068,"d":"0.10"},{"v":0.11593631868367563,"d":"0.12"},{"v":0.11593631868367563,"d":"0.12"},{"v":0.652333693,"d":"0.65"}]
["51680","Lynchburg City","VA",{"v":0.156937809,"d":"0.16"},{"v":0.6457263788074846,"d":"0.65"},{"v":0.6457263788074846,"d":"0.65"},{"v":0.749660119,"d":"0.75"}]
["51683","Manassas City","VA",{"v":0.077852275,"d":"0.08"},{"v":8.9977272631462559E-4,"d":"0.00"},{"v":8.9977272631462559E-4,"d":"0.00"},{"v":0.5380652645,"d":"0.54"}]
["51685","Manassas Park City","VA",{"v":0.042224189,"d":"0.04"},{"v":1.7445870522964679E-6,"d":"0.00"},{"v":1.7445870522964677E-6,"d":"0.00"},{"v":0.51200488,"d":"0.51"}]
["51690","Martinsville City","VA",{"v":0.17331483399999997,"d":"0.17"},{"v":0.8736738364154072,"d":"0.87"},{"v":0.8736738364154072,"d":"0.87"},{"v":0.7785594285,"d":"0.78"}]
["51700","Newport News City","VA",{"v":0.129208475,"d":"0.13"},{"v":0.01269242990334297,"d":"0.01"},{"v":0.01269242990334297,"d":"0.01"},{"v":0.4829264770000001,"d":"0.48"}]
["51710","Norfolk City","VA",{"v":0.07160228399999999,"d":"0.07"},{"v":2.5998905574612941E-5,"d":"0.00"},{"v":2.5998905574612948E-5,"d":"0.00"},{"v":0.38459424799999997,"d":"0.38"}]
["51720","Norton City","VA",{"v":0.21195620400000004,"d":"0.21"},{"v":2.0280113433164004,"d":"2.03"},{"v":2.0280113433164004,"d":"2.03"},{"v":0.8837300254999999,"d":"0.88"}]
["51730","Petersburg City","VA",{"v":0.177818166,"d":"0.18"},{"v":0.609675506133108,"d":"0.61"},{"v":0.6096755061331081,"d":"0.61"},{"v":0.697324148,"d":"0.70"}]
["51735","Poquoson City","VA",{"v":0.252467274,"d":"0.25"},{"v":1.6873923072949983,"d":"1.69"},{"v":1.6873923072949983,"d":"1.69"},{"v":0.5410278565,"d":"0.54"}]
["51740","Portsmouth City","VA",{"v":0.120609235,"d":"0.12"},{"v":5.0929443409352395E-3,"d":"0.01"},{"v":0.005092944340935239,"d":"0.01"},{"v":0.495285274,"d":"0.50"}]
["51750","Radford","VA",{"v":0.146874608,"d":"0.15"},{"v":0.7344958886333971,"d":"0.73"},{"v":0.7344958886333972,"d":"0.73"},{"v":0.6245892404999999,"d":"0.62"}]
["51760","Richmond City","VA",{"v":0.084518108,"d":"0.08"},{"v":9.1780034943399959E-5,"d":"0.00"},{"v":9.1780034943399945E-5,"d":"0.00"},{"v":0.5471385435,"d":"0.55"}]
["51770","Roanoke City","VA",{"v":0.126680768,"d":"0.13"},{"v":0.013807963358337762,"d":"0.01"},{"v":0.013807963358337765,"d":"0.01"},{"v":0.628745476,"d":"0.63"}]
["51775","Salem City","VA",{"v":0.147051381,"d":"0.15"},{"v":0.25807908783647804,"d":"0.26"},{"v":0.2580790878364779,"d":"0.26"},{"v":0.6926917199999999,"d":"0.69"}]
["51790","Staunton City","VA",{"v":0.189543522,"d":"0.19"},{"v":0.8631976834112204,"d":"0.86"},{"v":0.8631976834112203,"d":"0.86"},{"v":0.626121185,"d":"0.63"}]
["51800","Suffolk City","VA",{"v":0.277055709,"d":"0.28"},{"v":1.927612305152699,"d":"1.93"},{"v":1.9276123051526988,"d":"1.93"},{"v":0.8068188454999999,"d":"0.81"}]
["51810","Virginia Beach City","VA",{"v":0.18535133899999998,"d":"0.19"},{"v":0.29073380086899103,"d":"0.29"},{"v":0.29073380086899103,"d":"0.29"},{"v":0.5078245079999999,"d":"0.51"}]
["51820","Waynesboro City","VA",{"v":0.171909966,"d":"0.17"},{"v":0.5145214304062491,"d":"0.51"},{"v":0.5145214304062491,"d":"0.51"},{"v":0.7041818269999999,"d":"0.70"}]
["51830","Williamsburg City","VA",{"v":0.17268934,"d":"0.17"},{"v":0.9120378339717271,"d":"0.91"},{"v":0.9120378339717273,"d":"0.91"},{"v":0.7002724785000001,"d":"0.70"}]
["51840","Winchester City","VA",{"v":0.11610909800000001,"d":"0.12"},{"v":0.003256084354178727,"d":"0.00"},{"v":3.2560843541787265E-3,"d":"0.00"},{"v":0.5195556695,"d":"0.52"}]
["53001","Adams","WA",{"v":0.41591679,"d":"0.42"},{"v":2.605878219291304,"d":"2.61"},{"v":2.605878219291304,"d":"2.61"},{"v":1.3499999999999999,"d":"1.35"}]
["53003","Asotin","WA",{"v":0.362898881,"d":"0.36"},{"v":2.565697468804044,"d":"2.57"},{"v":2.565697468804044,"d":"2.57"},{"v":1.3499999999999999,"d":"1.35"}]
["53005","Benton","WA",{"v":0.360348744,"d":"0.36"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":1.3499999999999999,"d":"1.35"}]
["53007","Chelan","WA",{"v":0.336796963,"d":"0.34"},{"v":3.020043451096784,"d":"3.02"},{"v":3.020043451096784,"d":"3.02"},{"v":2.1999999999999997,"d":"2.20"}]
["53009","Clallam","WA",{"v":0.351571163,"d":"0.35"},{"v":2.819443224710728,"d":"2.82"},{"v":2.8194432247107284,"d":"2.82"},{"v":2.000291479820628,"d":"2.00"}]
["53011","Clark","WA",{"v":0.271652348,"d":"0.27"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.000291479820628,"d":"2.00"}]
["53013","Columbia","WA",{"v":0.388504628,"d":"0.39"},{"v":2.766699569600839,"d":"2.77"},{"v":2.766699569600839,"d":"2.77"},{"v":2.1999999999999997,"d":"2.20"}]
["53015","Cowlitz","WA",{"v":0.32483615099999996,"d":"0.32"},{"v":2.819396742762727,"d":"2.82"},{"v":2.819396742762727,"d":"2.82"},{"v":2.000291479820628,"d":"2.00"}]
["53017","Douglas","WA",{"v":0.384138203,"d":"0.38"},{"v":2.777938491983806,"d":"2.78"},{"v":2.7779384919838055,"d":"2.78"},{"v":2.1999999999999997,"d":"2.20"}]
["53019","Ferry","WA",{"v":0.408926918,"d":"0.41"},{"v":3.1059514008676703,"d":"3.11"},{"v":3.1059514008676703,"d":"3.11"},{"v":2.1999999999999997,"d":"2.20"}]
["53021","Franklin","WA",{"v":0.375002278,"d":"0.38"},{"v":2.590542813739835,"d":"2.59"},{"v":2.5905428137398356,"d":"2.59"},{"v":1.3499999999999996,"d":"1.35"}]
["53023","Garfield","WA",{"v":0.473223676,"d":"0.47"},{"v":2.7824446186149445,"d":"2.78"},{"v":2.782444618614945,"d":"2.78"},{"v":1.3499999999999999,"d":"1.35"}]
["53025","Grant","WA",{"v":0.40539291800000005,"d":"0.41"},{"v":2.6871691299720397,"d":"2.69"},{"v":2.6871691299720393,"d":"2.69"},{"v":1.3499999999999999,"d":"1.35"}]
["53027","Grays Harbor","WA",{"v":0.347682493,"d":"0.35"},{"v":2.7832017042202466,"d":"2.78"},{"v":2.783201704220247,"d":"2.78"},{"v":2.0002914798206284,"d":"2.00"}]
["53029","Island","WA",{"v":0.373814531,"d":"0.37"},{"v":2.5112526199248735,"d":"2.51"},{"v":2.511252619924873,"d":"2.51"},{"v":2.0002914798206275,"d":"2.00"}]
["53031","Jefferson","WA",{"v":0.368226098,"d":"0.37"},{"v":2.857489892218295,"d":"2.86"},{"v":2.857489892218295,"d":"2.86"},{"v":2.000291479820628,"d":"2.00"}]
["53033","King","WA",{"v":0.225166599,"d":"0.23"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":1.3307399103139015,"d":"1.33"}]
["53035","Kitsap","WA",{"v":0.292558207,"d":"0.29"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":1.754304932735426,"d":"1.75"}]
["53037","Kittitas","WA",{"v":0.36373438,"d":"0.36"},{"v":2.944512625213863,"d":"2.94"},{"v":2.9445126252138625,"d":"2.94"},2.05]
["53039","Klickitat","WA",{"v":0.411954667,"d":"0.41"},{"v":2.644558575737518,"d":"2.64"},{"v":2.644558575737518,"d":"2.64"},{"v":2.1999999999999997,"d":"2.20"}]
["53041","Lewis","WA",{"v":0.3599080250000001,"d":"0.36"},{"v":2.8672181159472245,"d":"2.87"},{"v":2.867218115947225,"d":"2.87"},{"v":2.000291479820628,"d":"2.00"}]
["53043","Lincoln","WA",{"v":0.465887587,"d":"0.47"},{"v":2.791359157892281,"d":"2.79"},{"v":2.7913591578922814,"d":"2.79"},{"v":1.3499999999999999,"d":"1.35"}]
["53045","Mason","WA",{"v":0.376001834,"d":"0.38"},{"v":2.844148571844136,"d":"2.84"},{"v":2.8441485718441357,"d":"2.84"},{"v":2.0002914798206275,"d":"2.00"}]
["53047","Okanogan","WA",{"v":0.41110119200000006,"d":"0.41"},{"v":2.9042318401811325,"d":"2.90"},{"v":2.9042318401811325,"d":"2.90"},{"v":2.1999999999999997,"d":"2.20"}]
["53049","Pacific","WA",{"v":0.385506092,"d":"0.39"},{"v":2.8278717082399742,"d":"2.83"},{"v":2.8278717082399742,"d":"2.83"},{"v":2.000291479820628,"d":"2.00"}]
["53051","Pend Oreille","WA",{"v":0.374009406,"d":"0.37"},{"v":3.154731378237268,"d":"3.15"},{"v":3.1547313782372686,"d":"3.15"},{"v":2.1999999999999997,"d":"2.20"}]
["53053","Pierce","WA",{"v":0.28112813500000006,"d":"0.28"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":1.5599103139013455,"d":"1.56"}]
["53055","San Juan","WA",{"v":0.466325894,"d":"0.47"},{"v":2.6075388137051814,"d":"2.61"},{"v":2.6075388137051814,"d":"2.61"},{"v":2.000291479820628,"d":"2.00"}]
["53057","Skagit","WA",{"v":0.346992324,"d":"0.35"},{"v":2.646754874801324,"d":"2.65"},{"v":2.646754874801324,"d":"2.65"},{"v":2.0002914798206275,"d":"2.00"}]
["53059","Skamania","WA",{"v":0.382186367,"d":"0.38"},{"v":3.14332168885182,"d":"3.14"},{"v":3.1433216888518203,"d":"3.14"},{"v":2.000291479820628,"d":"2.00"}]
["53061","Snohomish","WA",{"v":0.290901385,"d":"0.29"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.57567264573991,"d":"2.58"}]
["53063","Spokane","WA",{"v":0.31587990199999993,"d":"0.32"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.1999999999999997,"d":"2.20"}]
["53065","Stevens","WA",{"v":0.384772405,"d":"0.38"},{"v":3.0428372144144853,"d":"3.04"},{"v":3.0428372144144857,"d":"3.04"},{"v":2.1999999999999997,"d":"2.20"}]
["53067","Thurston","WA",{"v":0.312941437,"d":"0.31"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.000291479820628,"d":"2.00"}]
["53069","Wahkiakum","WA",{"v":0.416837401,"d":"0.42"},{"v":2.8603169215016786,"d":"2.86"},{"v":2.8603169215016777,"d":"2.86"},{"v":2.000291479820628,"d":"2.00"}]
["53071","Walla Walla","WA",{"v":0.380020605,"d":"0.38"},{"v":2.522992203001711,"d":"2.52"},{"v":2.5229922030017105,"d":"2.52"},{"v":2.1999999999999997,"d":"2.20"}]
["53073","Whatcom","WA",{"v":0.321048998,"d":"0.32"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.0002914798206275,"d":"2.00"}]
["53075","Whitman","WA",{"v":0.369069633,"d":"0.37"},{"v":2.5780058739690173,"d":"2.58"},{"v":2.5780058739690173,"d":"2.58"},{"v":1.3499999999999999,"d":"1.35"}]
["53077","Yakima","WA",{"v":0.36485606100000006,"d":"0.36"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":2.1999999999999997,"d":"2.20"}]
["54001","Barbour","WV",{"v":0.8347966020000002,"d":"0.83"},{"v":5.67873549630354,"d":"5.68"},{"v":5.67873549630354,"d":"5.68"},{"v":2.7983746429999994,"d":"2.80"}]
["54003","Berkeley","WV",{"v":0.736639547,"d":"0.74"},{"v":5.950115733909303,"d":"5.95"},{"v":5.950115733909305,"d":"5.95"},{"v":2.1893034429999996,"d":"2.19"}]
["54005","Boone","WV",{"v":0.823051753,"d":"0.82"},{"v":5.8196601235240575,"d":"5.82"},{"v":5.8196601235240575,"d":"5.82"},{"v":2.798474243,"d":"2.80"}]
["54007","Braxton","WV",{"v":0.858787078,"d":"0.86"},{"v":5.86843902674066,"d":"5.87"},{"v":5.868439026740659,"d":"5.87"},{"v":3.0188260284999995,"d":"3.02"}]
["54009","Brooke","WV",{"v":0.730755317,"d":"0.73"},{"v":5.356801132905753,"d":"5.36"},{"v":5.356801132905753,"d":"5.36"},{"v":2.2838247425000002,"d":"2.28"}]
["54011","Cabell","WV",{"v":0.648229821,"d":"0.65"},{"v":5.208107243803632,"d":"5.21"},{"v":5.208107243803632,"d":"5.21"},{"v":2.348239493,"d":"2.35"}]
["54013","Calhoun","WV",{"v":0.8543095730000001,"d":"0.85"},{"v":5.506988026608244,"d":"5.51"},{"v":5.506988026608245,"d":"5.51"},{"v":3.053846556,"d":"3.05"}]
["54015","Clay","WV",{"v":0.8515826269999999,"d":"0.85"},{"v":5.764344164597311,"d":"5.76"},{"v":5.764344164597311,"d":"5.76"},{"v":3.0181294965,"d":"3.02"}]
["54017","Doddridge","WV",{"v":0.864279379,"d":"0.86"},{"v":5.387670108352002,"d":"5.39"},{"v":5.387670108352001,"d":"5.39"},{"v":3.0022333554999996,"d":"3.00"}]
["54019","Fayette","WV",{"v":0.7457524019999999,"d":"0.75"},{"v":6.018513014394047,"d":"6.02"},{"v":6.018513014394047,"d":"6.02"},{"v":2.8963476294999992,"d":"2.90"}]
["54021","Gilmer","WV",{"v":0.801681151,"d":"0.80"},{"v":5.4637823627805036,"d":"5.46"},{"v":5.463782362780504,"d":"5.46"},{"v":2.9472463510000004,"d":"2.95"}]
["54023","Grant","WV",{"v":0.833319832,"d":"0.83"},{"v":6.203857177970183,"d":"6.20"},{"v":6.203857177970183,"d":"6.20"},{"v":2.756046923,"d":"2.76"}]
["54025","Greenbrier","WV",{"v":0.7949717569999999,"d":"0.79"},{"v":6.193059859830836,"d":"6.19"},{"v":6.193059859830836,"d":"6.19"},{"v":2.8439001034999998,"d":"2.84"}]
["54027","Hampshire","WV",{"v":0.8657001010000002,"d":"0.87"},{"v":6.218437115110206,"d":"6.22"},{"v":6.218437115110206,"d":"6.22"},{"v":2.9246137635,"d":"2.92"}]
["54029","Hancock","WV",{"v":0.690863114,"d":"0.69"},{"v":5.29713131977187,"d":"5.30"},{"v":5.29713131977187,"d":"5.30"},{"v":2.2521126045,"d":"2.25"}]
["54031","Hardy","WV",{"v":0.8139377030000001,"d":"0.81"},{"v":6.22127686075127,"d":"6.22"},{"v":6.22127686075127,"d":"6.22"},{"v":2.930936827,"d":"2.93"}]
["54033","Harrison","WV",{"v":0.727222374,"d":"0.73"},{"v":5.25702582588308,"d":"5.26"},{"v":5.25702582588308,"d":"5.26"},{"v":2.4853946524999997,"d":"2.49"}]
["54035","Jackson","WV",{"v":0.828336146,"d":"0.83"},{"v":5.633493815480695,"d":"5.63"},{"v":5.633493815480695,"d":"5.63"},{"v":2.6715362630000006,"d":"2.67"}]
["54037","Jefferson","WV",{"v":0.8094544029999999,"d":"0.81"},{"v":5.875305181052482,"d":"5.88"},{"v":5.875305181052483,"d":"5.88"},{"v":2.0827490075,"d":"2.08"}]
["54039","Kanawha","WV",{"v":0.677885765,"d":"0.68"},{"v":5.378584013497325,"d":"5.38"},{"v":5.378584013497325,"d":"5.38"},{"v":2.614307962,"d":"2.61"}]
["54041","Lewis","WV",{"v":0.7862032059999999,"d":"0.79"},{"v":5.510581414944775,"d":"5.51"},{"v":5.510581414944775,"d":"5.51"},{"v":2.8124798425,"d":"2.81"}]
["54043","Lincoln","WV",{"v":0.866900774,"d":"0.87"},{"v":5.718540908609064,"d":"5.72"},{"v":5.718540908609064,"d":"5.72"},{"v":2.8793290445000004,"d":"2.88"}]
["54045","Logan","WV",{"v":0.7946060280000001,"d":"0.79"},{"v":5.814213813172545,"d":"5.81"},{"v":5.814213813172545,"d":"5.81"},{"v":2.7651075235000007,"d":"2.77"}]
["54047","McDowell","WV",{"v":0.8240274640000002,"d":"0.82"},{"v":6.210705400571972,"d":"6.21"},{"v":6.210705400571973,"d":"6.21"},{"v":3.0382451465,"d":"3.04"}]
["54049","Marion","WV",{"v":0.72957605,"d":"0.73"},{"v":5.284615897747867,"d":"5.28"},{"v":5.284615897747866,"d":"5.28"},{"v":2.546380863,"d":"2.55"}]
["54051","Marshall","WV",{"v":0.7705245859999998,"d":"0.77"},{"v":5.609682719820473,"d":"5.61"},{"v":5.609682719820473,"d":"5.61"},{"v":2.5116337399999997,"d":"2.51"}]
["54053","Mason","WV",{"v":0.822234235,"d":"0.82"},{"v":5.825633499713993,"d":"5.83"},{"v":5.825633499713993,"d":"5.83"},{"v":2.500919986,"d":"2.50"}]
["54055","Mercer","WV",{"v":0.714351627,"d":"0.71"},{"v":5.941066064621734,"d":"5.94"},{"v":5.941066064621733,"d":"5.94"},{"v":2.6226682674999995,"d":"2.62"}]
["54057","Mineral","WV",{"v":0.7924952140000001,"d":"0.79"},{"v":5.935788627944176,"d":"5.94"},{"v":5.935788627944177,"d":"5.94"},{"v":2.7416292999999996,"d":"2.74"}]
["54059","Mingo","WV",{"v":0.8243524580000002,"d":"0.82"},{"v":6.0174012724179065,"d":"6.02"},{"v":6.0174012724179065,"d":"6.02"},{"v":2.835513543,"d":"2.84"}]
["54061","Monongalia","WV",{"v":0.65667115,"d":"0.66"},{"v":5.471095281500251,"d":"5.47"},{"v":5.471095281500251,"d":"5.47"},{"v":2.393038082,"d":"2.39"}]
["54063","Monroe","WV",{"v":0.8628939769999999,"d":"0.86"},{"v":6.0951264684404105,"d":"6.10"},{"v":6.0951264684404105,"d":"6.10"},{"v":2.774451791,"d":"2.77"}]
["54065","Morgan","WV",{"v":0.8564867469999999,"d":"0.86"},{"v":6.187812424099554,"d":"6.19"},{"v":6.187812424099554,"d":"6.19"},{"v":2.961986185,"d":"2.96"}]
["54067","Nicholas","WV",{"v":0.8097901709999998,"d":"0.81"},{"v":6.276378004762993,"d":"6.28"},{"v":6.276378004762994,"d":"6.28"},{"v":2.9307608974999995,"d":"2.93"}]
["54069","Ohio","WV",{"v":0.66453966,"d":"0.66"},{"v":5.158642595020679,"d":"5.16"},{"v":5.1586425950206785,"d":"5.16"},{"v":2.178346313,"d":"2.18"}]
["54071","Pendleton","WV",{"v":0.875193328,"d":"0.88"},{"v":6.26853087645266,"d":"6.27"},{"v":6.26853087645266,"d":"6.27"},{"v":3.0178134300000004,"d":"3.02"}]
["54073","Pleasants","WV",{"v":0.759503947,"d":"0.76"},{"v":5.567236322000768,"d":"5.57"},{"v":5.567236322000768,"d":"5.57"},{"v":2.8008220600000002,"d":"2.80"}]
["54075","Pocahontas","WV",{"v":0.8111839179999999,"d":"0.81"},{"v":6.504662547645008,"d":"6.50"},{"v":6.504662547645009,"d":"6.50"},{"v":3.1660860195000002,"d":"3.17"}]
["54077","Preston","WV",{"v":0.834294742,"d":"0.83"},{"v":6.240145843247975,"d":"6.24"},{"v":6.240145843247975,"d":"6.24"},{"v":2.8783612930000007,"d":"2.88"}]
["54079","Putnam","WV",{"v":0.731372729,"d":"0.73"},{"v":5.658883959720896,"d":"5.66"},{"v":5.658883959720896,"d":"5.66"},{"v":2.4834773090000004,"d":"2.48"}]
["54081","Raleigh","WV",{"v":0.7094672069999999,"d":"0.71"},{"v":6.008263855296583,"d":"6.01"},{"v":6.008263855296583,"d":"6.01"},{"v":2.6902356239999996,"d":"2.69"}]
["54083","Randolph","WV",{"v":0.756632873,"d":"0.76"},{"v":6.053440894226041,"d":"6.05"},{"v":6.053440894226041,"d":"6.05"},{"v":2.99830835,"d":"3.00"}]
["54085","Ritchie","WV",{"v":0.8642057839999999,"d":"0.86"},{"v":5.368404614401179,"d":"5.37"},{"v":5.368404614401179,"d":"5.37"},{"v":2.9849972504999998,"d":"2.98"}]
["54087","Roane","WV",{"v":0.82552361,"d":"0.83"},{"v":5.440244947112179,"d":"5.44"},{"v":5.440244947112179,"d":"5.44"},{"v":2.9064118145,"d":"2.91"}]
["54089","Summers","WV",{"v":0.821490046,"d":"0.82"},{"v":5.991855558221735,"d":"5.99"},{"v":5.991855558221735,"d":"5.99"},{"v":2.864037591,"d":"2.86"}]
["54091","Taylor","WV",{"v":0.774177548,"d":"0.77"},{"v":5.565982017248043,"d":"5.57"},{"v":5.565982017248043,"d":"5.57"},{"v":2.6473506520000005,"d":"2.65"}]
["54093","Tucker","WV",{"v":0.8454700190000001,"d":"0.85"},{"v":5.8869666172073085,"d":"5.89"},{"v":5.8869666172073085,"d":"5.89"},{"v":3.0996008135000004,"d":"3.10"}]
["54095","Tyler","WV",{"v":0.84683047,"d":"0.85"},{"v":5.461586053651329,"d":"5.46"},{"v":5.461586053651327,"d":"5.46"},{"v":2.9171602990000003,"d":"2.92"}]
["54097","Upshur","WV",{"v":0.782472516,"d":"0.78"},{"v":5.717493139678687,"d":"5.72"},{"v":5.717493139678687,"d":"5.72"},{"v":2.7984108410000004,"d":"2.80"}]
["54099","Wayne","WV",{"v":0.7755574240000002,"d":"0.78"},{"v":5.623515483384927,"d":"5.62"},{"v":5.623515483384926,"d":"5.62"},{"v":2.795788864,"d":"2.80"}]
["54101","Webster","WV",{"v":0.8201870709999999,"d":"0.82"},{"v":6.553908318735111,"d":"6.55"},{"v":6.55390831873511,"d":"6.55"},{"v":3.2310616430000003,"d":"3.23"}]
["54103","Wetzel","WV",{"v":0.763538064,"d":"0.76"},{"v":5.427925462174402,"d":"5.43"},{"v":5.427925462174402,"d":"5.43"},{"v":2.8309288560000003,"d":"2.83"}]
["54105","Wirt","WV",{"v":0.8607743880000001,"d":"0.86"},{"v":5.756158917157938,"d":"5.76"},{"v":5.756158917157937,"d":"5.76"},{"v":2.9501872445,"d":"2.95"}]
["54107","Wood","WV",{"v":0.695866557,"d":"0.70"},{"v":5.262388814149592,"d":"5.26"},{"v":5.262388814149592,"d":"5.26"},{"v":2.3904277560000002,"d":"2.39"}]
["54109","Wyoming","WV",{"v":0.824056504,"d":"0.82"},{"v":6.0324485831438714,"d":"6.03"},{"v":6.0324485831438714,"d":"6.03"},{"v":2.9751628515,"d":"2.98"}]
["55001","Adams","WI",{"v":0.450224378,"d":"0.45"},{"v":3.3990168815190196,"d":"3.40"},{"v":3.39901688151902,"d":"3.40"},{"v":1.2420853449999998,"d":"1.24"}]
["55003","Ashland","WI",{"v":0.37635619200000003,"d":"0.38"},{"v":3.417439131870122,"d":"3.42"},{"v":3.417439131870121,"d":"3.42"},{"v":1.3075495265000001,"d":"1.31"}]
["55005","Barron","WI",{"v":0.40596770599999993,"d":"0.41"},{"v":3.3979112807932133,"d":"3.40"},{"v":3.3979112807932133,"d":"3.40"},{"v":1.1931962580000002,"d":"1.19"}]
["55007","Bayfield","WI",{"v":0.427069025,"d":"0.43"},{"v":3.5952814237389665,"d":"3.60"},{"v":3.595281423738966,"d":"3.60"},{"v":1.4217289854999997,"d":"1.42"}]
["55009","Brown","WI",{"v":0.32383636900000007,"d":"0.32"},{"v":2.8255676381070676,"d":"2.83"},{"v":2.8255676381070676,"d":"2.83"},{"v":0.9048649675000001,"d":"0.90"}]
["55011","Buffalo","WI",{"v":0.449772107,"d":"0.45"},{"v":3.3809716471761377,"d":"3.38"},{"v":3.3809716471761377,"d":"3.38"},{"v":1.2911704975,"d":"1.29"}]
["55013","Burnett","WI",{"v":0.440679595,"d":"0.44"},{"v":3.550972741212629,"d":"3.55"},{"v":3.5509727412126284,"d":"3.55"},{"v":1.3195395445,"d":"1.32"}]
["55015","Calumet","WI",{"v":0.38480593799999996,"d":"0.38"},{"v":3.0085379227790554,"d":"3.01"},{"v":3.0085379227790554,"d":"3.01"},{"v":0.9594246659999999,"d":"0.96"}]
["55017","Chippewa","WI",{"v":0.386758159,"d":"0.39"},{"v":3.3872911761139166,"d":"3.39"},{"v":3.3872911761139166,"d":"3.39"},{"v":1.1608072070000002,"d":"1.16"}]
["55019","Clark","WI",{"v":0.432092348,"d":"0.43"},{"v":3.488200520085434,"d":"3.49"},{"v":3.4882005200854334,"d":"3.49"},{"v":1.2815186629999997,"d":"1.28"}]
["55021","Columbia","WI",{"v":0.43038104800000004,"d":"0.43"},{"v":3.0740812539108293,"d":"3.07"},{"v":3.0740812539108293,"d":"3.07"},{"v":1.063397574,"d":"1.06"}]
["55023","Crawford","WI",{"v":0.40796526299999997,"d":"0.41"},{"v":3.2149608621458228,"d":"3.21"},{"v":3.2149608621458228,"d":"3.21"},{"v":1.2238658725,"d":"1.22"}]
["55025","Dane","WI",{"v":0.325612134,"d":"0.33"},{"v":2.863892055841537,"d":"2.86"},{"v":2.863892055841537,"d":"2.86"},{"v":0.8876487044999998,"d":"0.89"}]
["55027","Dodge","WI",{"v":0.417552159,"d":"0.42"},{"v":2.9870710943573444,"d":"2.99"},{"v":2.9870710943573444,"d":"2.99"},{"v":0.9905842689999999,"d":"0.99"}]
["55029","Door","WI",{"v":0.43674833699999993,"d":"0.44"},{"v":3.1334137591858857,"d":"3.13"},{"v":3.1334137591858857,"d":"3.13"},{"v":1.0686727694999998,"d":"1.07"}]
["55031","Douglas","WI",{"v":0.36425417599999993,"d":"0.36"},{"v":3.3964679659002717,"d":"3.40"},{"v":3.396467965900272,"d":"3.40"},{"v":1.2357306940000001,"d":"1.24"}]
["55033","Dunn","WI",{"v":0.41391577300000004,"d":"0.41"},{"v":3.2902609606148085,"d":"3.29"},{"v":3.290260960614809,"d":"3.29"},{"v":1.1461954134999999,"d":"1.15"}]
["55035","Eau Claire","WI",{"v":0.35287241299999994,"d":"0.35"},{"v":3.277688226052024,"d":"3.28"},{"v":3.277688226052024,"d":"3.28"},{"v":1.1048434294999998,"d":"1.10"}]
["55037","Florence","WI",{"v":0.413034983,"d":"0.41"},{"v":3.562356186276787,"d":"3.56"},{"v":3.562356186276788,"d":"3.56"},{"v":1.53912665,"d":"1.54"}]
["55039","Fond Du Lac","WI",{"v":0.38930821500000007,"d":"0.39"},{"v":3.0262277638410864,"d":"3.03"},{"v":3.026227763841086,"d":"3.03"},{"v":0.969446905,"d":"0.97"}]
["55041","Forest","WI",{"v":0.41314624000000005,"d":"0.41"},{"v":3.5796562205555755,"d":"3.58"},{"v":3.5796562205555755,"d":"3.58"},{"v":1.5303080950000003,"d":"1.53"}]
["55043","Grant","WI",{"v":0.4277544569999999,"d":"0.43"},{"v":3.09577085516188,"d":"3.10"},{"v":3.09577085516188,"d":"3.10"},{"v":1.1085570515,"d":"1.11"}]
["55045","Green","WI",{"v":0.43466129299999995,"d":"0.43"},{"v":3.0261866981233467,"d":"3.03"},{"v":3.0261866981233467,"d":"3.03"},{"v":1.0277364605,"d":"1.03"}]
["55047","Green Lake","WI",{"v":0.445042343,"d":"0.45"},{"v":3.134399364602466,"d":"3.13"},{"v":3.134399364602466,"d":"3.13"},{"v":1.0883435435000002,"d":"1.09"}]
["55049","Iowa","WI",{"v":0.44581464700000006,"d":"0.45"},{"v":3.1280570206423075,"d":"3.13"},{"v":3.128057020642307,"d":"3.13"},{"v":1.162896873,"d":"1.16"}]
["55051","Iron","WI",{"v":0.38004809400000006,"d":"0.38"},{"v":3.538727654907899,"d":"3.54"},{"v":3.5387276549079,"d":"3.54"},{"v":1.444421031,"d":"1.44"}]
["55053","Jackson","WI",{"v":0.41275093200000007,"d":"0.41"},{"v":3.3629503104163065,"d":"3.36"},{"v":3.3629503104163065,"d":"3.36"},{"v":1.2706485435,"d":"1.27"}]
["55055","Jefferson","WI",{"v":0.398745944,"d":"0.40"},{"v":2.9903799648344984,"d":"2.99"},{"v":2.9903799648344984,"d":"2.99"},{"v":0.971241935,"d":"0.97"}]
["55057","Juneau","WI",{"v":0.430736205,"d":"0.43"},{"v":3.339080128036734,"d":"3.34"},{"v":3.339080128036734,"d":"3.34"},{"v":1.2208784645,"d":"1.22"}]
["55059","Kenosha","WI",{"v":0.31415702200000006,"d":"0.31"},{"v":2.6624838736182723,"d":"2.66"},{"v":2.6624838736182723,"d":"2.66"},{"v":0.8629284435000001,"d":"0.86"}]
["55061","Kewaunee","WI",{"v":0.43957101300000007,"d":"0.44"},{"v":3.132010583533132,"d":"3.13"},{"v":3.132010583533132,"d":"3.13"},{"v":1.0706216315,"d":"1.07"}]
["55063","La Crosse","WI",{"v":0.331665193,"d":"0.33"},{"v":3.126123251364365,"d":"3.13"},{"v":3.1261232513643646,"d":"3.13"},{"v":1.069942481,"d":"1.07"}]
["55065","Lafayette","WI",{"v":0.49015788799999993,"d":"0.49"},{"v":3.1202315611925733,"d":"3.12"},{"v":3.120231561192573,"d":"3.12"},{"v":1.09317459,"d":"1.09"}]
["55067","Langlade","WI",{"v":0.37280639499999996,"d":"0.37"},{"v":3.4125577113770356,"d":"3.41"},{"v":3.412557711377036,"d":"3.41"},{"v":1.3939312955,"d":"1.39"}]
["55069","Lincoln","WI",{"v":0.3644344179999999,"d":"0.36"},{"v":3.4679698154332415,"d":"3.47"},{"v":3.467969815433241,"d":"3.47"},{"v":1.3741838220000002,"d":"1.37"}]
["55071","Manitowoc","WI",{"v":0.39011704499999994,"d":"0.39"},{"v":2.935702696352375,"d":"2.94"},{"v":2.935702696352375,"d":"2.94"},{"v":1.0118895565000001,"d":"1.01"}]
["55073","Marathon","WI",{"v":0.366046198,"d":"0.37"},{"v":3.3414931134819628,"d":"3.34"},{"v":3.3414931134819628,"d":"3.34"},{"v":1.1888740779999998,"d":"1.19"}]
["55075","Marinette","WI",{"v":0.37895587000000003,"d":"0.38"},{"v":3.466139093210435,"d":"3.47"},{"v":3.466139093210435,"d":"3.47"},{"v":1.3592598985000002,"d":"1.36"}]
["55077","Marquette","WI",{"v":0.46189580900000005,"d":"0.46"},{"v":3.2881742586855327,"d":"3.29"},{"v":3.2881742586855323,"d":"3.29"},{"v":1.2146360044999998,"d":"1.21"}]
["55078","Menominee","WI",{"v":0.409985957,"d":"0.41"},{"v":3.696205932055221,"d":"3.70"},{"v":3.696205932055221,"d":"3.70"},{"v":1.5681224040000001,"d":"1.57"}]
["55079","Milwaukee","WI",{"v":0.101449054,"d":"0.10"},{"v":5.0135912455081178E-5,"d":"0.00"},{"v":5.0135912455081178E-5,"d":"0.00"},{"v":0.6227255465,"d":"0.62"}]
["55081","Monroe","WI",{"v":0.399100432,"d":"0.40"},{"v":3.276120392424591,"d":"3.28"},{"v":3.276120392424591,"d":"3.28"},{"v":1.177476099,"d":"1.18"}]
["55083","Oconto","WI",{"v":0.4104329769999999,"d":"0.41"},{"v":3.4461557698345633,"d":"3.45"},{"v":3.4461557698345637,"d":"3.45"},{"v":1.3182814499999997,"d":"1.32"}]
["55085","Oneida","WI",{"v":0.394713962,"d":"0.39"},{"v":3.4590367468284686,"d":"3.46"},{"v":3.4590367468284686,"d":"3.46"},{"v":1.377882587,"d":"1.38"}]
["55087","Outagamie","WI",{"v":0.356149736,"d":"0.36"},{"v":2.9529320666117886,"d":"2.95"},{"v":2.9529320666117886,"d":"2.95"},{"v":0.9655981069999998,"d":"0.97"}]
["55089","Ozaukee","WI",{"v":0.361958703,"d":"0.36"},{"v":2.878681030752206,"d":"2.88"},{"v":2.878681030752206,"d":"2.88"},{"v":0.9139103230000001,"d":"0.91"}]
["55091","Pepin","WI",{"v":0.45537751800000004,"d":"0.46"},{"v":3.3334999767799958,"d":"3.33"},{"v":3.333499976779996,"d":"3.33"},{"v":1.2259306415,"d":"1.23"}]
["55093","Pierce","WI",{"v":0.41331536900000004,"d":"0.41"},{"v":3.256101720235317,"d":"3.26"},{"v":3.256101720235317,"d":"3.26"},{"v":1.089749525,"d":"1.09"}]
["55095","Polk","WI",{"v":0.42608373299999996,"d":"0.43"},{"v":3.481709932067687,"d":"3.48"},{"v":3.4817099320676865,"d":"3.48"},{"v":1.2462413795,"d":"1.25"}]
["55097","Portage","WI",{"v":0.3769305439999999,"d":"0.38"},{"v":3.1579983728130085,"d":"3.16"},{"v":3.1579983728130077,"d":"3.16"},{"v":1.101227005,"d":"1.10"}]
["55099","Price","WI",{"v":0.416920051,"d":"0.42"},{"v":3.578781297773613,"d":"3.58"},{"v":3.578781297773613,"d":"3.58"},{"v":1.4803388684999998,"d":"1.48"}]
["55101","Racine","WI",{"v":0.321079518,"d":"0.32"},{"v":2.652121160162481,"d":"2.65"},{"v":2.652121160162481,"d":"2.65"},{"v":0.8691178724999998,"d":"0.87"}]
["55103","Richland","WI",{"v":0.4179909030000001,"d":"0.42"},{"v":3.211255480328093,"d":"3.21"},{"v":3.2112554803280937,"d":"3.21"},{"v":1.2108017285000001,"d":"1.21"}]
["55105","Rock","WI",{"v":0.378007238,"d":"0.38"},{"v":2.933991207521176,"d":"2.93"},{"v":2.933991207521176,"d":"2.93"},{"v":0.9113295344999998,"d":"0.91"}]
["55107","Rusk","WI",{"v":0.400709277,"d":"0.40"},{"v":3.5599448870892014,"d":"3.56"},{"v":3.5599448870892014,"d":"3.56"},{"v":1.3662218565000002,"d":"1.37"}]
["55109","St Croix","WI",{"v":0.421181209,"d":"0.42"},{"v":3.204536597967587,"d":"3.20"},{"v":3.204536597967587,"d":"3.20"},{"v":1.0422485150000003,"d":"1.04"}]
["55111","Sauk","WI",{"v":0.38975776900000003,"d":"0.39"},{"v":3.0794041969455908,"d":"3.08"},{"v":3.079404196945591,"d":"3.08"},{"v":1.110202207,"d":"1.11"}]
["55113","Sawyer","WI",{"v":0.39881691999999996,"d":"0.40"},{"v":3.621578035278427,"d":"3.62"},{"v":3.6215780352784277,"d":"3.62"},{"v":1.4817321055,"d":"1.48"}]
["55115","Shawano","WI",{"v":0.4024434290000001,"d":"0.40"},{"v":3.3926026924005357,"d":"3.39"},{"v":3.3926026924005357,"d":"3.39"},{"v":1.292529817,"d":"1.29"}]
["55117","Sheboygan","WI",{"v":0.36920224500000004,"d":"0.37"},{"v":2.8679547155227363,"d":"2.87"},{"v":2.8679547155227363,"d":"2.87"},{"v":0.9862362545,"d":"0.99"}]
["55119","Taylor","WI",{"v":0.401249257,"d":"0.40"},{"v":3.5529051701042835,"d":"3.55"},{"v":3.5529051701042835,"d":"3.55"},{"v":1.361690938,"d":"1.36"}]
["55121","Trempealeau","WI",{"v":0.43917608299999994,"d":"0.44"},{"v":3.2393294169828177,"d":"3.24"},{"v":3.2393294169828173,"d":"3.24"},{"v":1.2400419050000002,"d":"1.24"}]
["55123","Vernon","WI",{"v":0.43918069299999996,"d":"0.44"},{"v":3.2348015217791932,"d":"3.23"},{"v":3.2348015217791932,"d":"3.23"},{"v":1.207419362,"d":"1.21"}]
["55125","Vilas","WI",{"v":0.41985836500000007,"d":"0.42"},{"v":3.5217743383794113,"d":"3.52"},{"v":3.5217743383794113,"d":"3.52"},{"v":1.4499737355000002,"d":"1.45"}]
["55127","Walworth","WI",{"v":0.39060583800000004,"d":"0.39"},{"v":2.928408031750707,"d":"2.93"},{"v":2.928408031750707,"d":"2.93"},{"v":0.9762998340000001,"d":"0.98"}]
["55129","Washburn","WI",{"v":0.40952331099999995,"d":"0.41"},{"v":3.5716059573243237,"d":"3.57"},{"v":3.5716059573243237,"d":"3.57"},{"v":1.3857045249999997,"d":"1.39"}]
["55131","Washington","WI",{"v":0.371403035,"d":"0.37"},{"v":2.9223269565480274,"d":"2.92"},{"v":2.9223269565480274,"d":"2.92"},{"v":0.9704064605000003,"d":"0.97"}]
["55133","Waukesha","WI",{"v":0.30142802100000005,"d":"0.30"},{"v":2.6326785284600502,"d":"2.63"},{"v":2.63267852846005,"d":"2.63"},{"v":0.8821379715000002,"d":"0.88"}]
["55135","Waupaca","WI",{"v":0.401800369,"d":"0.40"},{"v":3.240173167586752,"d":"3.24"},{"v":3.240173167586751,"d":"3.24"},{"v":1.2110579825,"d":"1.21"}]
["55137","Waushara","WI",{"v":0.44381582,"d":"0.44"},{"v":3.299149099659848,"d":"3.30"},{"v":3.299149099659848,"d":"3.30"},{"v":1.213165926,"d":"1.21"}]
["55139","Winnebago","WI",{"v":0.33959031600000006,"d":"0.34"},{"v":2.859670933936586,"d":"2.86"},{"v":2.8596709339365853,"d":"2.86"},{"v":0.8814996399999998,"d":"0.88"}]
["55141","Wood","WI",{"v":0.37660822399999994,"d":"0.38"},{"v":3.140031621683775,"d":"3.14"},{"v":3.140031621683775,"d":"3.14"},{"v":1.0928082485,"d":"1.09"}]
["56001","Albany","WY",{"v":0.20899982799999997,"d":"0.21"},{"v":1.7060389805501208,"d":"1.71"},{"v":1.706038980550121,"d":"1.71"},{"v":0.5033017359999999,"d":"0.50"}]
["56003","Big Horn","WY",{"v":0.26503335,"d":"0.27"},{"v":1.7444720804693779,"d":"1.74"},{"v":1.7444720804693774,"d":"1.74"},{"v":0.6102877440000002,"d":"0.61"}]
["56005","Campbell","WY",{"v":0.22406732799999998,"d":"0.22"},{"v":1.7672734473639107,"d":"1.77"},{"v":1.7672734473639107,"d":"1.77"},{"v":0.5160753164999999,"d":"0.52"}]
["56007","Carbon","WY",{"v":0.229712145,"d":"0.23"},{"v":1.7617636155332121,"d":"1.76"},{"v":1.7617636155332124,"d":"1.76"},{"v":0.5558075815,"d":"0.56"}]
["56009","Converse","WY",{"v":0.24816489499999997,"d":"0.25"},{"v":1.707590637892268,"d":"1.71"},{"v":1.7075906378922678,"d":"1.71"},{"v":0.5402521839999999,"d":"0.54"}]
["56011","Crook","WY",{"v":0.264809788,"d":"0.26"},{"v":1.8369198115628045,"d":"1.84"},{"v":1.8369198115628045,"d":"1.84"},{"v":0.621749665,"d":"0.62"}]
["56013","Fremont","WY",{"v":0.232620512,"d":"0.23"},{"v":1.797883883519911,"d":"1.80"},{"v":1.7978838835199111,"d":"1.80"},{"v":0.562643968,"d":"0.56"}]
["56015","Goshen","WY",{"v":0.238957922,"d":"0.24"},{"v":1.671206812865591,"d":"1.67"},{"v":1.6712068128655908,"d":"1.67"},{"v":0.520933261,"d":"0.52"}]
["56017","Hot Springs","WY",{"v":0.22208594299999998,"d":"0.22"},{"v":1.7415962703338996,"d":"1.74"},{"v":1.7415962703338994,"d":"1.74"},{"v":0.528256802,"d":"0.53"}]
["56019","Johnson","WY",{"v":0.232483924,"d":"0.23"},{"v":1.7367444631652318,"d":"1.74"},{"v":1.7367444631652316,"d":"1.74"},{"v":0.558601389,"d":"0.56"}]
["56021","Laramie","WY",{"v":0.229197579,"d":"0.23"},{"v":1.6392891406274086,"d":"1.64"},{"v":1.6392891406274086,"d":"1.64"},{"v":0.482518947,"d":"0.48"}]
["56023","Lincoln","WY",{"v":0.250049895,"d":"0.25"},{"v":1.8406127260181573,"d":"1.84"},{"v":1.8406127260181568,"d":"1.84"},{"v":0.6148860185000001,"d":"0.61"}]
["56025","Natrona","WY",{"v":0.21756054800000002,"d":"0.22"},{"v":1.6350842209525607,"d":"1.64"},{"v":1.6350842209525607,"d":"1.64"},{"v":0.47857608150000014,"d":"0.48"}]
["56027","Niobrara","WY",{"v":0.27235323,"d":"0.27"},{"v":1.728824800799592,"d":"1.73"},{"v":1.7288248007995923,"d":"1.73"},{"v":0.5846248910000001,"d":"0.58"}]
["56029","Park","WY",{"v":0.23273320500000003,"d":"0.23"},{"v":1.7643999079107484,"d":"1.76"},{"v":1.7643999079107484,"d":"1.76"},{"v":0.5708302525,"d":"0.57"}]
["56031","Platte","WY",{"v":0.24746130499999996,"d":"0.25"},{"v":1.6939494900936394,"d":"1.69"},{"v":1.6939494900936394,"d":"1.69"},{"v":0.544162978,"d":"0.54"}]
["56033","Sheridan","WY",{"v":0.223532455,"d":"0.22"},{"v":1.7365463712357376,"d":"1.74"},{"v":1.7365463712357379,"d":"1.74"},{"v":0.5479136124999999,"d":"0.55"}]
["56035","Sublette","WY",{"v":0.262124861,"d":"0.26"},{"v":1.8284056956417731,"d":"1.83"},{"v":1.828405695641773,"d":"1.83"},{"v":0.6276247330000001,"d":"0.63"}]
["56037","Sweetwater","WY",{"v":0.21257019000000002,"d":"0.21"},{"v":1.7298954047755923,"d":"1.73"},{"v":1.7298954047755926,"d":"1.73"},{"v":0.4944339394999999,"d":"0.49"}]
["56039","Teton","WY",{"v":0.214437195,"d":"0.21"},{"v":1.9723834209929316,"d":"1.97"},{"v":1.9723834209929316,"d":"1.97"},{"v":0.6481722870000001,"d":"0.65"}]
["56041","Uinta","WY",{"v":0.22510646899999998,"d":"0.23"},{"v":1.8078464371384249,"d":"1.81"},{"v":1.8078464371384246,"d":"1.81"},{"v":0.5540146300000002,"d":"0.55"}]
["56043","Washakie","WY",{"v":0.23152177000000002,"d":"0.23"},{"v":1.7309832983531122,"d":"1.73"},{"v":1.7309832983531122,"d":"1.73"},{"v":0.5308234780000002,"d":"0.53"}]
["56045","Weston","WY",{"v":0.23801905699999998,"d":"0.24"},{"v":1.7420121522242902,"d":"1.74"},{"v":1.74201215222429,"d":"1.74"},{"v":0.5497481635000001,"d":"0.55"}]
["Grand Total",null,null,{"v":0.32219854638862844,"d":"0.32"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]

{"sheet":"dropdown","index":8,"n_rows":6,"n_cols":3,"rows_kept":6}
["old stove options",null,"new stove options"]
["Uncertified",null,"Non-catalytic"]
["Certified-20 years or older",null,"Catalytic"]
[null,null,"Hybrid"]
[null,null,"Non-wood (gas or electric)"]
[null,null,"Pellet"]

{"sheet":"pellet-burnrate","index":9,"n_rows":3147,"n_cols":6,"rows_kept":3147}
[]
[]
["Average of Burn rate - TONS WOOD PER APPLIANCE PER COUNTY",null,null,"Appliance Type"]
["StateAndCountyFIPSCode","CountyName","PostalStateCode","Furnace-Pellet","Pellet Hydronic Heater","Pellet Woodstove"]
["01001","Autauga","AL",{"v":1.5536744971091483,"d":"1.55"},{"v":1.5536744971091485,"d":"1.55"},{"v":0.197752255,"d":"0.20"}]
["01003","Baldwin","AL",{"v":1.4234910034685844,"d":"1.42"},{"v":1.4234910034685841,"d":"1.42"},{"v":0.14681418,"d":"0.15"}]
["01005","Barbour","AL",{"v":1.5529623161264818,"d":"1.55"},{"v":1.5529623161264818,"d":"1.55"},{"v":0.232790737,"d":"0.23"}]
["01007","Bibb","AL",{"v":1.6934745098300792,"d":"1.69"},{"v":1.6934745098300794,"d":"1.69"},{"v":0.311246967,"d":"0.31"}]
["01009","Blount","AL",{"v":1.7238413160666186,"d":"1.72"},{"v":1.7238413160666184,"d":"1.72"},{"v":0.300073947,"d":"0.30"}]
["01011","Bullock","AL",{"v":1.5180563483329486,"d":"1.52"},{"v":1.5180563483329488,"d":"1.52"},{"v":0.24014011200000002,"d":"0.24"}]
["01013","Butler","AL",{"v":1.4963986901775024,"d":"1.50"},{"v":1.4963986901775026,"d":"1.50"},{"v":0.243304185,"d":"0.24"}]
["01015","Calhoun","AL",{"v":1.580059075389058,"d":"1.58"},{"v":1.5800590753890582,"d":"1.58"},{"v":0.223085641,"d":"0.22"}]
["01017","Chambers","AL",{"v":1.4622324220629637,"d":"1.46"},{"v":1.4622324220629637,"d":"1.46"},{"v":0.251899752,"d":"0.25"}]
["01019","Cherokee","AL",{"v":1.7073384004621672,"d":"1.71"},{"v":1.7073384004621672,"d":"1.71"},{"v":0.249633745,"d":"0.25"}]
["01021","Chilton","AL",{"v":1.6271190791234236,"d":"1.63"},{"v":1.6271190791234236,"d":"1.63"},{"v":0.292158877,"d":"0.29"}]
["01023","Choctaw","AL",{"v":1.5932258481993844,"d":"1.59"},{"v":1.5932258481993844,"d":"1.59"},{"v":0.301075338,"d":"0.30"}]
["01025","Clarke","AL",{"v":1.5155356693953812,"d":"1.52"},{"v":1.5155356693953814,"d":"1.52"},{"v":0.244535303,"d":"0.24"}]
["01027","Clay","AL",{"v":1.552582620004964,"d":"1.55"},{"v":1.5525826200049642,"d":"1.55"},{"v":0.312733201,"d":"0.31"}]
["01029","Cleburne","AL",{"v":1.5536145271025417,"d":"1.55"},{"v":1.5536145271025414,"d":"1.55"},{"v":0.346570527,"d":"0.35"}]
["01031","Coffee","AL",{"v":1.4798621674087598,"d":"1.48"},{"v":1.4798621674087598,"d":"1.48"},{"v":0.188115011,"d":"0.19"}]
["01033","Colbert","AL",{"v":1.6124778150214287,"d":"1.61"},{"v":1.6124778150214287,"d":"1.61"},{"v":0.212065725,"d":"0.21"}]
["01035","Conecuh","AL",{"v":1.5335768659372155,"d":"1.53"},{"v":1.5335768659372158,"d":"1.53"},{"v":0.23849049799999997,"d":"0.24"}]
["01037","Coosa","AL",{"v":1.6882185519999702,"d":"1.69"},{"v":1.6882185519999702,"d":"1.69"},{"v":0.33639114,"d":"0.34"}]
["01039","Covington","AL",{"v":1.5347223965977306,"d":"1.53"},{"v":1.5347223965977306,"d":"1.53"},{"v":0.204932362,"d":"0.20"}]
["01041","Crenshaw","AL",{"v":1.5302707034441905,"d":"1.53"},{"v":1.5302707034441903,"d":"1.53"},{"v":0.247673309,"d":"0.25"}]
["01043","Cullman","AL",{"v":1.6447517301522943,"d":"1.64"},{"v":1.644751730152294,"d":"1.64"},{"v":0.260635366,"d":"0.26"}]
["01045","Dale","AL",{"v":1.5214129792963158,"d":"1.52"},{"v":1.521412979296316,"d":"1.52"},{"v":0.19974491,"d":"0.20"}]
["01047","Dallas","AL",{"v":1.4744312085160274,"d":"1.47"},{"v":1.4744312085160278,"d":"1.47"},{"v":0.172443183,"d":"0.17"}]
["01049","De Kalb","AL",{"v":1.6403724043977093,"d":"1.64"},{"v":1.6403724043977093,"d":"1.64"},{"v":0.272753965,"d":"0.27"}]
["01051","Elmore","AL",{"v":1.5679698353226097,"d":"1.57"},{"v":1.5679698353226095,"d":"1.57"},{"v":0.239331974,"d":"0.24"}]
["01053","Escambia","AL",{"v":1.5534538971454872,"d":"1.55"},{"v":1.5534538971454872,"d":"1.55"},{"v":0.201470765,"d":"0.20"}]
["01055","Etowah","AL",{"v":1.4939791487905973,"d":"1.49"},{"v":1.4939791487905976,"d":"1.49"},{"v":0.191943253,"d":"0.19"}]
["01057","Fayette","AL",{"v":1.598830196004467,"d":"1.60"},{"v":1.5988301960044669,"d":"1.60"},{"v":0.306342374,"d":"0.31"}]
["01059","Franklin","AL",{"v":1.6166585253710408,"d":"1.62"},{"v":1.6166585253710406,"d":"1.62"},{"v":0.256404797,"d":"0.26"}]
["01061","Geneva","AL",{"v":1.483413953287815,"d":"1.48"},{"v":1.4834139532878148,"d":"1.48"},{"v":0.193181429,"d":"0.19"}]
["01063","Greene","AL",{"v":1.649806433280382,"d":"1.65"},{"v":1.649806433280382,"d":"1.65"},{"v":0.267276476,"d":"0.27"}]
["01065","Hale","AL",{"v":1.681461340634846,"d":"1.68"},{"v":1.681461340634846,"d":"1.68"},{"v":0.233575876,"d":"0.23"}]
["01067","Henry","AL",{"v":1.628971824449626,"d":"1.63"},{"v":1.628971824449626,"d":"1.63"},{"v":0.205637921,"d":"0.21"}]
["01069","Houston","AL",{"v":1.4194295346262125,"d":"1.42"},{"v":1.4194295346262125,"d":"1.42"},{"v":0.151058486,"d":"0.15"}]
["01071","Jackson","AL",{"v":1.7622660394599199,"d":"1.76"},{"v":1.7622660394599197,"d":"1.76"},{"v":0.287620314,"d":"0.29"}]
["01073","Jefferson","AL",{"v":1.4619869621161174,"d":"1.46"},{"v":1.4619869621161177,"d":"1.46"},{"v":0.222839666,"d":"0.22"}]
["01075","Lamar","AL",{"v":1.5398512632998613,"d":"1.54"},{"v":1.5398512632998613,"d":"1.54"},{"v":0.303390691,"d":"0.30"}]
["01077","Lauderdale","AL",{"v":1.703000928851186,"d":"1.70"},{"v":1.7030009288511863,"d":"1.70"},{"v":0.200581324,"d":"0.20"}]
["01079","Lawrence","AL",{"v":1.615537177628587,"d":"1.62"},{"v":1.6155371776285867,"d":"1.62"},{"v":0.256190852,"d":"0.26"}]
["01081","Lee","AL",{"v":1.4150710010561212,"d":"1.42"},{"v":1.4150710010561214,"d":"1.42"},{"v":0.237140285,"d":"0.24"}]
["01083","Limestone","AL",{"v":1.6892233520081312,"d":"1.69"},{"v":1.6892233520081312,"d":"1.69"},{"v":0.206829392,"d":"0.21"}]
["01085","Lowndes","AL",{"v":1.5902730339239033,"d":"1.59"},{"v":1.5902730339239035,"d":"1.59"},{"v":0.259220974,"d":"0.26"}]
["01087","Macon","AL",{"v":1.572230943141355,"d":"1.57"},{"v":1.5722309431413553,"d":"1.57"},{"v":0.206181561,"d":"0.21"}]
["01089","Madison","AL",{"v":1.4015380591598918,"d":"1.40"},{"v":1.4015380591598918,"d":"1.40"},{"v":0.200039829,"d":"0.20"}]
["01091","Marengo","AL",{"v":1.4965650216971407,"d":"1.50"},{"v":1.4965650216971407,"d":"1.50"},{"v":0.23713760199999998,"d":"0.24"}]
["01093","Marion","AL",{"v":1.5258124165977835,"d":"1.53"},{"v":1.5258124165977835,"d":"1.53"},{"v":0.251604577,"d":"0.25"}]
["01095","Marshall","AL",{"v":1.719511869421587,"d":"1.72"},{"v":1.7195118694215872,"d":"1.72"},{"v":0.20957707099999998,"d":"0.21"}]
["01097","Mobile","AL",{"v":1.303896441081565,"d":"1.30"},{"v":1.303896441081565,"d":"1.30"},{"v":0.119315807,"d":"0.12"}]
["01099","Monroe","AL",{"v":1.569817207129303,"d":"1.57"},{"v":1.5698172071293028,"d":"1.57"},{"v":0.24560257999999996,"d":"0.25"}]
["01101","Montgomery","AL",{"v":1.399819629230355,"d":"1.40"},{"v":1.3998196292303549,"d":"1.40"},{"v":0.131950855,"d":"0.13"}]
["01103","Morgan","AL",{"v":1.7340232011595287,"d":"1.73"},{"v":1.7340232011595285,"d":"1.73"},{"v":0.216427138,"d":"0.22"}]
["01105","Perry","AL",{"v":1.518929783429055,"d":"1.52"},{"v":1.5189297834290552,"d":"1.52"},{"v":0.244792241,"d":"0.24"}]
["01107","Pickens","AL",{"v":1.5369251156471893,"d":"1.54"},{"v":1.5369251156471893,"d":"1.54"},{"v":0.312654965,"d":"0.31"}]
["01109","Pike","AL",{"v":1.556794891361908,"d":"1.56"},{"v":1.556794891361908,"d":"1.56"},{"v":0.209202769,"d":"0.21"}]
["01111","Randolph","AL",{"v":1.5932600147384433,"d":"1.59"},{"v":1.5932600147384433,"d":"1.59"},{"v":0.284844099,"d":"0.28"}]
["01113","Russell","AL",{"v":1.4194407503288649,"d":"1.42"},{"v":1.4194407503288649,"d":"1.42"},{"v":0.189635768,"d":"0.19"}]
["01115","St Clair","AL",{"v":1.6821519476405873,"d":"1.68"},{"v":1.682151947640587,"d":"1.68"},{"v":0.269034357,"d":"0.27"}]
["01117","Shelby","AL",{"v":1.532826438955122,"d":"1.53"},{"v":1.532826438955122,"d":"1.53"},{"v":0.20306286,"d":"0.20"}]
["01119","Sumter","AL",{"v":1.6032983184013463,"d":"1.60"},{"v":1.603298318401346,"d":"1.60"},{"v":0.277108018,"d":"0.28"}]
["01121","Talladega","AL",{"v":1.5912368155810412,"d":"1.59"},{"v":1.591236815581041,"d":"1.59"},{"v":0.249710732,"d":"0.25"}]
["01123","Tallapoosa","AL",{"v":1.5701938356483325,"d":"1.57"},{"v":1.5701938356483327,"d":"1.57"},{"v":0.277677101,"d":"0.28"}]
["01125","Tuscaloosa","AL",{"v":1.5284615801082844,"d":"1.53"},{"v":1.5284615801082846,"d":"1.53"},{"v":0.224041354,"d":"0.22"}]
["01127","Walker","AL",{"v":1.7193631829298246,"d":"1.72"},{"v":1.7193631829298244,"d":"1.72"},{"v":0.297645618,"d":"0.30"}]
["01129","Washington","AL",{"v":1.5665600040651073,"d":"1.57"},{"v":1.566560004065107,"d":"1.57"},{"v":0.276626817,"d":"0.28"}]
["01131","Wilcox","AL",{"v":1.6154738065238274,"d":"1.62"},{"v":1.6154738065238272,"d":"1.62"},{"v":0.267857136,"d":"0.27"}]
["01133","Winston","AL",{"v":1.6296952261763185,"d":"1.63"},{"v":1.6296952261763185,"d":"1.63"},{"v":0.294783249,"d":"0.29"}]
["02013","Aleutians East","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02016","Aleutians West","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02020","Anchorage","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},0.25]
["02050","Bethel","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02060","Bristol Bay","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02068","Denali","AK",{"v":6.732,"d":"6.73"},{"v":6.732000000000001,"d":"6.73"},0.25]
["02070","Dillingham","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02090","Fairbanks North Star","AK",{"v":6.732,"d":"6.73"},{"v":6.732,"d":"6.73"},0.25]
["02100","Haines","AK",{"v":3.3659999999999997,"d":"3.37"},{"v":3.3660000000000005,"d":"3.37"},0.25]
["02105","Hoonah Angoon","AK",{"v":3.366,"d":"3.37"},{"v":3.366,"d":"3.37"},0.25]
["02110","Juneau","AK",{"v":3.366,"d":"3.37"},{"v":3.3659999999999997,"d":"3.37"},0.25]
["02122","Kenai Peninsula","AK",{"v":5.049,"d":"5.05"},{"v":5.049,"d":"5.05"},{"v":0,"d":"0.00"}]
["02130","Ketchikan Gateway","AK",{"v":3.366,"d":"3.37"},{"v":3.3660000000000005,"d":"3.37"},0.25]
["02150","Kodiak Island","AK",{"v":5.049,"d":"5.05"},{"v":5.049000000000001,"d":"5.05"},{"v":0,"d":"0.00"}]
["02158","Kusilvak","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02164","Lake and Peninsula","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02170","Matanuska Susitna","AK",{"v":5.0489999999999995,"d":"5.05"},{"v":5.0489999999999995,"d":"5.05"},0.25]
["02180","Nome","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02185","North Slope","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02188","Northwest Arctic","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02195","Petersburg","AK",{"v":3.366,"d":"3.37"},{"v":3.366,"d":"3.37"},0.25]
["02198","Prince of Wales-Hyder","AK",{"v":3.366,"d":"3.37"},{"v":3.366,"d":"3.37"},0.25]
["02220","Sitka","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["02230","Skagway","AK",{"v":3.3660000000000005,"d":"3.37"},{"v":3.366,"d":"3.37"},0.25]
["02240","Southeast Fairbanks","AK",{"v":6.732000000000001,"d":"6.73"},{"v":6.732,"d":"6.73"},0.25]
["02261","Valdez Cordova","AK",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},0.25]
["02275","Wrangell","AK",{"v":3.366,"d":"3.37"},{"v":3.3660000000000005,"d":"3.37"},0.25]
["02282","Yakutat","AK",{"v":3.366,"d":"3.37"},{"v":3.366,"d":"3.37"},0.25]
["02290","Yukon Koyukuk","AK",{"v":6.732,"d":"6.73"},{"v":6.732,"d":"6.73"},{"$error":"#DIV/0!"}]
["04001","Apache","AZ",{"v":1.162870794019604,"d":"1.16"},{"v":1.1628707940196041,"d":"1.16"},{"v":0.21783420800000003,"d":"0.22"}]
["04003","Cochise","AZ",{"v":0.9690001295316225,"d":"0.97"},{"v":0.9690001295316224,"d":"0.97"},{"v":0.058794199,"d":"0.06"}]
["04005","Coconino","AZ",{"v":1.1161264654888268,"d":"1.12"},{"v":1.1161264654888268,"d":"1.12"},{"v":0.132795911,"d":"0.13"}]
["04007","Gila","AZ",{"v":1.038640624700845,"d":"1.04"},{"v":1.0386406247008453,"d":"1.04"},{"v":0.092012597,"d":"0.09"}]
["04009","Graham","AZ",{"v":0.9820056987477898,"d":"0.98"},{"v":0.9820056987477895,"d":"0.98"},{"v":0.062496156,"d":"0.06"}]
["04011","Greenlee","AZ",{"v":0.9456255758256276,"d":"0.95"},{"v":0.9456255758256276,"d":"0.95"},{"v":0.065931473,"d":"0.07"}]
["04012","La Paz","AZ",{"v":1.0412338599210895,"d":"1.04"},{"v":1.0412338599210897,"d":"1.04"},{"v":0.061430907,"d":"0.06"}]
["04013","Maricopa","AZ",{"v":0.918472218886589,"d":"0.92"},{"v":0.918472218886589,"d":"0.92"},{"v":0.050167945,"d":"0.05"}]
["04015","Mohave","AZ",{"v":1.0193609989505241,"d":"1.02"},{"v":1.0193609989505241,"d":"1.02"},{"v":0.067937947,"d":"0.07"}]
["04017","Navajo","AZ",{"v":1.1595905817441443,"d":"1.16"},{"v":1.1595905817441443,"d":"1.16"},{"v":0.166625508,"d":"0.17"}]
["04019","Pima","AZ",{"v":0.952648977788797,"d":"0.95"},{"v":0.952648977788797,"d":"0.95"},{"v":0.04755907,"d":"0.05"}]
["04021","Pinal","AZ",{"v":0.9442755941613222,"d":"0.94"},{"v":0.944275594161322,"d":"0.94"},{"v":0.046174554,"d":"0.05"}]
["04023","Santa Cruz","AZ",{"v":0.9707941525448511,"d":"0.97"},{"v":0.9707941525448509,"d":"0.97"},{"v":0.065488456,"d":"0.07"}]
["04025","Yavapai","AZ",{"v":1.0011503870829028,"d":"1.00"},{"v":1.0011503870829026,"d":"1.00"},{"v":0.073736544,"d":"0.07"}]
["04027","Yuma","AZ",{"v":0.986102563823934,"d":"0.99"},{"v":0.986102563823934,"d":"0.99"},{"v":0.04349577,"d":"0.04"}]
["05001","Arkansas","AR",{"v":3.4854814797231217,"d":"3.49"},{"v":3.485481479723122,"d":"3.49"},{"v":0.337711514,"d":"0.34"}]
["05003","Ashley","AR",{"v":3.610334904453729,"d":"3.61"},{"v":3.610334904453729,"d":"3.61"},{"v":0.459792855,"d":"0.46"}]
["05005","Baxter","AR",{"v":4.149261875779503,"d":"4.15"},{"v":4.149261875779502,"d":"4.15"},{"v":0.726061341,"d":"0.73"}]
["05007","Benton","AR",{"v":4.0478203506676556,"d":"4.05"},{"v":4.047820350667655,"d":"4.05"},{"v":0.49900771900000007,"d":"0.50"}]
["05009","Boone","AR",{"v":4.283501718495705,"d":"4.28"},{"v":4.283501718495706,"d":"4.28"},{"v":0.606216968,"d":"0.61"}]
["05011","Bradley","AR",{"v":3.644517248542155,"d":"3.64"},{"v":3.6445172485421544,"d":"3.64"},{"v":0.595178951,"d":"0.60"}]
["05013","Calhoun","AR",{"v":3.613167969967085,"d":"3.61"},{"v":3.613167969967085,"d":"3.61"},{"v":0.690244677,"d":"0.69"}]
["05015","Carroll","AR",{"v":4.292536763418841,"d":"4.29"},{"v":4.292536763418841,"d":"4.29"},{"v":0.717485073,"d":"0.72"}]
["05017","Chicot","AR",{"v":3.441263458422852,"d":"3.44"},{"v":3.4412634584228523,"d":"3.44"},{"v":0.291469899,"d":"0.29"}]
["05019","Clark","AR",{"v":3.541778480842493,"d":"3.54"},{"v":3.5417784808424932,"d":"3.54"},{"v":0.565190471,"d":"0.57"}]
["05021","Clay","AR",{"v":3.789950282818702,"d":"3.79"},{"v":3.789950282818702,"d":"3.79"},{"v":0.347821113,"d":"0.35"}]
["05023","Cleburne","AR",{"v":4.031146505672221,"d":"4.03"},{"v":4.031146505672221,"d":"4.03"},{"v":0.811815886,"d":"0.81"}]
["05025","Cleveland","AR",{"v":3.825493700362675,"d":"3.83"},{"v":3.8254937003626748,"d":"3.83"},{"v":0.815062775,"d":"0.82"}]
["05027","Columbia","AR",{"v":3.512291748567431,"d":"3.51"},{"v":3.512291748567431,"d":"3.51"},{"v":0.592673475,"d":"0.59"}]
["05029","Conway","AR",{"v":3.4279273252865416,"d":"3.43"},{"v":3.427927325286541,"d":"3.43"},{"v":0.558023377,"d":"0.56"}]
["05031","Craighead","AR",{"v":3.6747012001716843,"d":"3.67"},{"v":3.674701200171684,"d":"3.67"},{"v":0.326755759,"d":"0.33"}]
["05033","Crawford","AR",{"v":3.809689618744967,"d":"3.81"},{"v":3.8096896187449665,"d":"3.81"},{"v":0.593440465,"d":"0.59"}]
["05035","Crittenden","AR",{"v":3.204782755886982,"d":"3.20"},{"v":3.2047827558869826,"d":"3.20"},{"v":0.230365926,"d":"0.23"}]
["05037","Cross","AR",{"v":4.074160741747844,"d":"4.07"},{"v":4.074160741747844,"d":"4.07"},{"v":0.340230699,"d":"0.34"}]
["05039","Dallas","AR",{"v":3.5474474196078662,"d":"3.55"},{"v":3.5474474196078662,"d":"3.55"},{"v":0.598256833,"d":"0.60"}]
["05041","Desha","AR",{"v":3.250070916011561,"d":"3.25"},{"v":3.2500709160115604,"d":"3.25"},{"v":0.282577062,"d":"0.28"}]
["05043","Drew","AR",{"v":3.729038113137346,"d":"3.73"},{"v":3.729038113137346,"d":"3.73"},{"v":0.508553782,"d":"0.51"}]
["05045","Faulkner","AR",{"v":3.7629786691030565,"d":"3.76"},{"v":3.762978669103056,"d":"3.76"},{"v":0.456145819,"d":"0.46"}]
["05047","Franklin","AR",{"v":4.0287364644430115,"d":"4.03"},{"v":4.0287364644430115,"d":"4.03"},{"v":0.580825325,"d":"0.58"}]
["05049","Fulton","AR",{"v":4.44990212621803,"d":"4.45"},{"v":4.4499021262180305,"d":"4.45"},{"v":0.807842946,"d":"0.81"}]
["05051","Garland","AR",{"v":3.7306728953093957,"d":"3.73"},{"v":3.7306728953093966,"d":"3.73"},{"v":0.618813054,"d":"0.62"}]
["05053","Grant","AR",{"v":3.588406499509572,"d":"3.59"},{"v":3.5884064995095715,"d":"3.59"},{"v":0.674398917,"d":"0.67"}]
["05055","Greene","AR",{"v":3.865259988005148,"d":"3.87"},{"v":3.8652599880051484,"d":"3.87"},{"v":0.428588973,"d":"0.43"}]
["05057","Hempstead","AR",{"v":3.396414683444842,"d":"3.40"},{"v":3.396414683444842,"d":"3.40"},{"v":0.444716801,"d":"0.44"}]
["05059","Hot Spring","AR",{"v":3.7446800999375784,"d":"3.74"},{"v":3.744680099937578,"d":"3.74"},{"v":0.677787926,"d":"0.68"}]
["05061","Howard","AR",{"v":3.518520841583139,"d":"3.52"},{"v":3.5185208415831384,"d":"3.52"},{"v":0.523983042,"d":"0.52"}]
["05063","Independence","AR",{"v":4.066932267548743,"d":"4.07"},{"v":4.066932267548743,"d":"4.07"},{"v":0.590264267,"d":"0.59"}]
["05065","Izard","AR",{"v":4.31895873377566,"d":"4.32"},{"v":4.31895873377566,"d":"4.32"},{"v":0.896032458,"d":"0.90"}]
["05067","Jackson","AR",{"v":3.2291964064543697,"d":"3.23"},{"v":3.2291964064543697,"d":"3.23"},{"v":0.333320519,"d":"0.33"}]
["05069","Jefferson","AR",{"v":3.657105432327745,"d":"3.66"},{"v":3.6571054323277457,"d":"3.66"},{"v":0.310764172,"d":"0.31"}]
["05071","Johnson","AR",{"v":4.012008040792151,"d":"4.01"},{"v":4.012008040792151,"d":"4.01"},{"v":0.746748049,"d":"0.75"}]
["05073","Lafayette","AR",{"v":3.535791519750857,"d":"3.54"},{"v":3.5357915197508576,"d":"3.54"},{"v":0.560371022,"d":"0.56"}]
["05075","Lawrence","AR",{"v":3.9232866937355313,"d":"3.92"},{"v":3.9232866937355313,"d":"3.92"},{"v":0.396816082,"d":"0.40"}]
["05077","Lee","AR",{"v":4.008389085161823,"d":"4.01"},{"v":4.008389085161822,"d":"4.01"},{"v":0.320128187,"d":"0.32"}]
["05079","Lincoln","AR",{"v":4.036623992148854,"d":"4.04"},{"v":4.036623992148854,"d":"4.04"},{"v":0.491164415,"d":"0.49"}]
["05081","Little River","AR",{"v":3.839407425393067,"d":"3.84"},{"v":3.8394074253930666,"d":"3.84"},{"v":0.49117575,"d":"0.49"}]
["05083","Logan","AR",{"v":3.8606816521667993,"d":"3.86"},{"v":3.8606816521667997,"d":"3.86"},{"v":0.600665968,"d":"0.60"}]
["05085","Lonoke","AR",{"v":3.5503191946987216,"d":"3.55"},{"v":3.5503191946987216,"d":"3.55"},{"v":0.340258992,"d":"0.34"}]
["05087","Madison","AR",{"v":4.325639213889376,"d":"4.33"},{"v":4.325639213889376,"d":"4.33"},{"v":0.921036518,"d":"0.92"}]
["05089","Marion","AR",{"v":4.426724352545725,"d":"4.43"},{"v":4.426724352545725,"d":"4.43"},{"v":0.835583281,"d":"0.84"}]
["05091","Miller","AR",{"v":3.5185039863885366,"d":"3.52"},{"v":3.5185039863885366,"d":"3.52"},{"v":0.382122399,"d":"0.38"}]
["05093","Mississippi","AR",{"v":2.3920712983322088,"d":"2.39"},{"v":2.392071298332209,"d":"2.39"},{"v":0.26688511,"d":"0.27"}]
["05095","Monroe","AR",{"v":3.5490968238200775,"d":"3.55"},{"v":3.549096823820078,"d":"3.55"},{"v":0.398627709,"d":"0.40"}]
["05097","Montgomery","AR",{"v":4.025134958327247,"d":"4.03"},{"v":4.025134958327248,"d":"4.03"},{"v":0.819009817,"d":"0.82"}]
["05099","Nevada","AR",{"v":3.6504631190018584,"d":"3.65"},{"v":3.650463119001858,"d":"3.65"},{"v":0.592595035,"d":"0.59"}]
["05101","Newton","AR",{"v":4.523462654904056,"d":"4.52"},{"v":4.523462654904056,"d":"4.52"},{"v":1.299370779,"d":"1.30"}]
["05103","Ouachita","AR",{"v":3.4625686442154877,"d":"3.46"},{"v":3.462568644215488,"d":"3.46"},{"v":0.56521908,"d":"0.57"}]
["05105","Perry","AR",{"v":3.87427919335026,"d":"3.87"},{"v":3.8742791933502603,"d":"3.87"},{"v":0.8586507100000002,"d":"0.86"}]
["05107","Phillips","AR",{"v":3.2692235023506093,"d":"3.27"},{"v":3.2692235023506093,"d":"3.27"},{"v":0.286146948,"d":"0.29"}]
["05109","Pike","AR",{"v":3.624438990057316,"d":"3.62"},{"v":3.6244389900573157,"d":"3.62"},{"v":0.653233743,"d":"0.65"}]
["05111","Poinsett","AR",{"v":3.6996380508565214,"d":"3.70"},{"v":3.6996380508565214,"d":"3.70"},{"v":0.354879905,"d":"0.35"}]
["05113","Polk","AR",{"v":4.044103014057323,"d":"4.04"},{"v":4.044103014057323,"d":"4.04"},{"v":0.797515177,"d":"0.80"}]
["05115","Pope","AR",{"v":3.852227842318178,"d":"3.85"},{"v":3.852227842318178,"d":"3.85"},{"v":0.6737057619999999,"d":"0.67"}]
["05117","Prairie","AR",{"v":3.5212222504015727,"d":"3.52"},{"v":3.5212222504015727,"d":"3.52"},{"v":0.44917346900000005,"d":"0.45"}]
["05119","Pulaski","AR",{"v":3.3286902572648946,"d":"3.33"},{"v":3.328690257264894,"d":"3.33"},{"v":0.420694642,"d":"0.42"}]
["05121","Randolph","AR",{"v":3.905719809853939,"d":"3.91"},{"v":3.905719809853939,"d":"3.91"},{"v":0.520782269,"d":"0.52"}]
["05123","St Francis","AR",{"v":3.810154312443925,"d":"3.81"},{"v":3.810154312443926,"d":"3.81"},{"v":0.339141165,"d":"0.34"}]
["05125","Saline","AR",{"v":3.4825777640721434,"d":"3.48"},{"v":3.482577764072143,"d":"3.48"},{"v":0.589706408,"d":"0.59"}]
["05127","Scott","AR",{"v":4.158964619556134,"d":"4.16"},{"v":4.158964619556134,"d":"4.16"},{"v":0.851593816,"d":"0.85"}]
["05129","Searcy","AR",{"v":4.513109809889786,"d":"4.51"},{"v":4.513109809889787,"d":"4.51"},{"v":1.001826444,"d":"1.00"}]
["05131","Sebastian","AR",{"v":2.8846067617929227,"d":"2.88"},{"v":2.8846067617929223,"d":"2.88"},{"v":0.393885406,"d":"0.39"}]
["05133","Sevier","AR",{"v":3.842330635079031,"d":"3.84"},{"v":3.8423306350790307,"d":"3.84"},{"v":0.591898737,"d":"0.59"}]
["05135","Sharp","AR",{"v":4.4573020943348345,"d":"4.46"},{"v":4.457302094334835,"d":"4.46"},{"v":0.928393986,"d":"0.93"}]
["05137","Stone","AR",{"v":4.327667968489572,"d":"4.33"},{"v":4.327667968489571,"d":"4.33"},{"v":1.07896788,"d":"1.08"}]
["05139","Union","AR",{"v":3.4762412141614063,"d":"3.48"},{"v":3.4762412141614063,"d":"3.48"},{"v":0.559168374,"d":"0.56"}]
["05141","Van Buren","AR",{"v":4.372054008115777,"d":"4.37"},{"v":4.372054008115777,"d":"4.37"},{"v":1.035298519,"d":"1.04"}]
["05143","Washington","AR",{"v":3.8791304170577807,"d":"3.88"},{"v":3.8791304170577803,"d":"3.88"},{"v":0.537643178,"d":"0.54"}]
["05145","White","AR",{"v":3.9102888529970263,"d":"3.91"},{"v":3.910288852997026,"d":"3.91"},{"v":0.528073326,"d":"0.53"}]
["05147","Woodruff","AR",{"v":3.866684151898406,"d":"3.87"},{"v":3.866684151898407,"d":"3.87"},{"v":0.364170191,"d":"0.36"}]
["05149","Yell","AR",{"v":3.93481960129239,"d":"3.93"},{"v":3.9348196012923897,"d":"3.93"},{"v":0.795490801,"d":"0.80"}]
["06001","Alameda","CA",{"v":0.16952816058980283,"d":"0.17"},{"v":0.16952816058980286,"d":"0.17"},{"v":0.47913707299999997,"d":"0.48"}]
["06003","Alpine","CA",{"v":3.8362729947854075,"d":"3.84"},{"v":3.8362729947854075,"d":"3.84"},{"v":1.390826559,"d":"1.39"}]
["06005","Amador","CA",{"v":3.114111682612899,"d":"3.11"},{"v":3.1141116826128994,"d":"3.11"},{"v":0.448594601,"d":"0.45"}]
["06007","Butte","CA",{"v":3.3175101116542045,"d":"3.32"},{"v":3.317510111654205,"d":"3.32"},{"v":0.431459436,"d":"0.43"}]
["06009","Calaveras","CA",{"v":3.1780843206875793,"d":"3.18"},{"v":3.1780843206875797,"d":"3.18"},{"v":0.502100546,"d":"0.50"}]
["06011","Colusa","CA",{"v":3.0897941087116974,"d":"3.09"},{"v":3.089794108711698,"d":"3.09"},{"v":0.321637291,"d":"0.32"}]
["06013","Contra Costa","CA",{"v":1.0731425882680072,"d":"1.07"},{"v":1.0731425882680072,"d":"1.07"},{"v":0.343060632,"d":"0.34"}]
["06015","Del Norte","CA",{"v":4.029806391595132,"d":"4.03"},{"v":4.029806391595131,"d":"4.03"},{"v":0.887252251,"d":"0.89"}]
["06017","El Dorado","CA",{"v":3.246636435946915,"d":"3.25"},{"v":3.246636435946915,"d":"3.25"},{"v":0.565357375,"d":"0.57"}]
["06019","Fresno","CA",{"v":2.8655073821638024,"d":"2.87"},{"v":2.8655073821638024,"d":"2.87"},{"v":0.250986085,"d":"0.25"}]
["06021","Glenn","CA",{"v":3.1035765568129983,"d":"3.10"},{"v":3.103576556812998,"d":"3.10"},{"v":0.408399438,"d":"0.41"}]
["06023","Humboldt","CA",{"v":3.2898677910923944,"d":"3.29"},{"v":3.289867791092394,"d":"3.29"},{"v":0.605316947,"d":"0.61"}]
["06025","Imperial","CA",{"v":2.8582627274685772,"d":"2.86"},{"v":2.8582627274685772,"d":"2.86"},{"v":0.158878373,"d":"0.16"}]
["06027","Inyo","CA",{"v":2.9560617938539115,"d":"2.96"},{"v":2.956061793853911,"d":"2.96"},{"v":0.214084112,"d":"0.21"}]
["06029","Kern","CA",{"v":2.821016345815366,"d":"2.82"},{"v":2.821016345815366,"d":"2.82"},{"v":0.19554839,"d":"0.20"}]
["06031","Kings","CA",{"v":2.7837302159009836,"d":"2.78"},{"v":2.7837302159009836,"d":"2.78"},{"v":0.185487802,"d":"0.19"}]
["06033","Lake","CA",{"v":3.3504471590738856,"d":"3.35"},{"v":3.350447159073886,"d":"3.35"},{"v":0.578532094,"d":"0.58"}]
["06035","Lassen","CA",{"v":3.4275108102748058,"d":"3.43"},{"v":3.427510810274805,"d":"3.43"},{"v":0.9816055549999999,"d":"0.98"}]
["06037","Los Angeles","CA",{"v":0.11479389050852407,"d":"0.11"},{"v":0.11479389050852407,"d":"0.11"},{"v":0.471302459,"d":"0.47"}]
["06039","Madera","CA",{"v":3.03331775531524,"d":"3.03"},{"v":3.0333177553152404,"d":"3.03"},{"v":0.368037395,"d":"0.37"}]
["06041","Marin","CA",{"v":2.9000732000409526,"d":"2.90"},{"v":2.900073200040953,"d":"2.90"},{"v":0.352454524,"d":"0.35"}]
["06043","Mariposa","CA",{"v":3.2095688441575474,"d":"3.21"},{"v":3.209568844157548,"d":"3.21"},{"v":0.565765667,"d":"0.57"}]
["06045","Mendocino","CA",{"v":3.326356518073906,"d":"3.33"},{"v":3.326356518073906,"d":"3.33"},{"v":0.694521622,"d":"0.69"}]
["06047","Merced","CA",{"v":2.9054588313936573,"d":"2.91"},{"v":2.9054588313936565,"d":"2.91"},{"v":0.23624124200000002,"d":"0.24"}]
["06049","Modoc","CA",{"v":3.1795334437993126,"d":"3.18"},{"v":3.1795334437993126,"d":"3.18"},{"v":0.511705773,"d":"0.51"}]
["06051","Mono","CA",{"v":3.710584983266542,"d":"3.71"},{"v":3.710584983266542,"d":"3.71"},{"v":0.884283733,"d":"0.88"}]
["06053","Monterey","CA",{"v":2.7915271166379876,"d":"2.79"},{"v":2.7915271166379876,"d":"2.79"},{"v":0.18758472,"d":"0.19"}]
["06055","Napa","CA",{"v":3.0548406346310726,"d":"3.05"},{"v":3.054840634631073,"d":"3.05"},{"v":0.363346449,"d":"0.36"}]
["06057","Nevada","CA",{"v":3.3564132103620863,"d":"3.36"},{"v":3.356413210362086,"d":"3.36"},{"v":0.598221746,"d":"0.60"}]
["06059","Orange","CA",{"v":9.2400690545641623E-4,"d":"0.00"},{"v":9.2400690545641623E-4,"d":"0.00"},{"v":1.065321202,"d":"1.07"}]
["06061","Placer","CA",{"v":3.0014663952667515,"d":"3.00"},{"v":3.001466395266751,"d":"3.00"},{"v":0.420557405,"d":"0.42"}]
["06063","Plumas","CA",{"v":3.192446415912621,"d":"3.19"},{"v":3.1924464159126207,"d":"3.19"},{"v":0.737469724,"d":"0.74"}]
["06065","Riverside","CA",{"v":2.8580959872001084,"d":"2.86"},{"v":2.858095987200108,"d":"2.86"},{"v":0.127546581,"d":"0.13"}]
["06067","Sacramento","CA",{"v":1.075705057552469,"d":"1.08"},{"v":1.075705057552469,"d":"1.08"},{"v":0.3917483929999999,"d":"0.39"}]
["06069","San Benito","CA",{"v":2.762135144221226,"d":"2.76"},{"v":2.7621351442212254,"d":"2.76"},{"v":0.178502444,"d":"0.18"}]
["06071","San Bernardino","CA",{"v":2.8338570866750237,"d":"2.83"},{"v":2.8338570866750237,"d":"2.83"},{"v":0.112623044,"d":"0.11"}]
["06073","San Diego","CA",{"v":2.528209961787523,"d":"2.53"},{"v":2.5282099617875224,"d":"2.53"},{"v":0.185274143,"d":"0.19"}]
["06075","San Francisco","CA",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["06077","San Joaquin","CA",{"v":2.7739099198233803,"d":"2.77"},{"v":2.7739099198233803,"d":"2.77"},{"v":0.262702986,"d":"0.26"}]
["06079","San Luis Obispo","CA",{"v":2.8331902461493943,"d":"2.83"},{"v":2.8331902461493943,"d":"2.83"},{"v":0.1635409,"d":"0.16"}]
["06081","San Mateo","CA",{"v":0.8267747385953425,"d":"0.83"},{"v":0.8267747385953425,"d":"0.83"},{"v":0.4347904,"d":"0.43"}]
["06083","Santa Barbara","CA",{"v":2.7164361454770307,"d":"2.72"},{"v":2.7164361454770307,"d":"2.72"},{"v":0.132567941,"d":"0.13"}]
["06085","Santa Clara","CA",{"v":1.479630853816803,"d":"1.48"},{"v":1.479630853816803,"d":"1.48"},{"v":0.38137325,"d":"0.38"}]
["06087","Santa Cruz","CA",{"v":2.6466600773159734,"d":"2.65"},{"v":2.646660077315973,"d":"2.65"},{"v":0.327807259,"d":"0.33"}]
["06089","Shasta","CA",{"v":3.167316560122093,"d":"3.17"},{"v":3.1673165601220927,"d":"3.17"},{"v":0.500121048,"d":"0.50"}]
["06091","Sierra","CA",{"v":3.337062935690879,"d":"3.34"},{"v":3.337062935690879,"d":"3.34"},{"v":0.753469606,"d":"0.75"}]
["06093","Siskiyou","CA",{"v":3.572733539654722,"d":"3.57"},{"v":3.572733539654722,"d":"3.57"},{"v":0.834540663,"d":"0.83"}]
["06095","Solano","CA",{"v":2.873110219432488,"d":"2.87"},{"v":2.8731102194324873,"d":"2.87"},{"v":0.279272815,"d":"0.28"}]
["06097","Sonoma","CA",{"v":3.039922121079132,"d":"3.04"},{"v":3.039922121079132,"d":"3.04"},{"v":0.410197838,"d":"0.41"}]
["06099","Stanislaus","CA",{"v":2.769651804424609,"d":"2.77"},{"v":2.7696518044246083,"d":"2.77"},{"v":0.246706853,"d":"0.25"}]
["06101","Sutter","CA",{"v":2.993909966628135,"d":"2.99"},{"v":2.9939099666281352,"d":"2.99"},{"v":0.276252211,"d":"0.28"}]
["06103","Tehama","CA",{"v":3.208353959448552,"d":"3.21"},{"v":3.2083539594485515,"d":"3.21"},{"v":0.484775756,"d":"0.48"}]
["06105","Trinity","CA",{"v":3.602389207669288,"d":"3.60"},{"v":3.602389207669288,"d":"3.60"},{"v":1.100148839,"d":"1.10"}]
["06107","Tulare","CA",{"v":2.840839230107428,"d":"2.84"},{"v":2.840839230107428,"d":"2.84"},{"v":0.250620089,"d":"0.25"}]
["06109","Tuolumne","CA",{"v":3.0754765783626357,"d":"3.08"},{"v":3.075476578362635,"d":"3.08"},{"v":0.475555962,"d":"0.48"}]
["06111","Ventura","CA",{"v":2.7155619131750544,"d":"2.72"},{"v":2.7155619131750535,"d":"2.72"},{"v":0.149664561,"d":"0.15"}]
["06113","Yolo","CA",{"v":3.014349384367334,"d":"3.01"},{"v":3.0143493843673337,"d":"3.01"},{"v":0.256654298,"d":"0.26"}]
["06115","Yuba","CA",{"v":3.146389830778156,"d":"3.15"},{"v":3.146389830778156,"d":"3.15"},{"v":0.43692482,"d":"0.44"}]
["08001","Adams","CO",{"v":2.5582170631077017,"d":"2.56"},{"v":2.5582170631077017,"d":"2.56"},{"v":0.397188516,"d":"0.40"}]
["08003","Alamosa","CO",{"v":2.794440931740162,"d":"2.79"},{"v":2.7944409317401626,"d":"2.79"},{"v":0.7266356,"d":"0.73"}]
["08005","Arapahoe","CO",{"v":2.316207008683215,"d":"2.32"},{"v":2.3162070086832145,"d":"2.32"},{"v":0.488629071,"d":"0.49"}]
["08007","Archuleta","CO",{"v":2.837465609529771,"d":"2.84"},{"v":2.8374656095297706,"d":"2.84"},{"v":0.9804044069999999,"d":"0.98"}]
["08009","Baca","CO",{"v":2.4964261249982305,"d":"2.50"},{"v":2.4964261249982305,"d":"2.50"},{"v":0.372414255,"d":"0.37"}]
["08011","Bent","CO",{"v":2.505250394950449,"d":"2.51"},{"v":2.5052503949504485,"d":"2.51"},{"v":0.314334412,"d":"0.31"}]
["08013","Boulder","CO",{"v":2.5365877323838486,"d":"2.54"},{"v":2.536587732383848,"d":"2.54"},{"v":0.579233669,"d":"0.58"}]
["08014","Broomfield","CO",{"v":0.13932150527884068,"d":"0.14"},{"v":0.13932150527884068,"d":"0.14"},{"v":0.927221094,"d":"0.93"}]
["08015","Chaffee","CO",{"v":2.5224744108875226,"d":"2.52"},{"v":2.522474410887523,"d":"2.52"},{"v":0.46145152000000006,"d":"0.46"}]
["08017","Cheyenne","CO",{"v":2.5755199474468453,"d":"2.58"},{"v":2.5755199474468453,"d":"2.58"},{"v":0.430771864,"d":"0.43"}]
["08019","Clear Creek","CO",{"v":2.7495434289691745,"d":"2.75"},{"v":2.7495434289691745,"d":"2.75"},{"v":0.930257584,"d":"0.93"}]
["08021","Conejos","CO",{"v":2.908085245811491,"d":"2.91"},{"v":2.908085245811491,"d":"2.91"},{"v":1.088074454,"d":"1.09"}]
["08023","Costilla","CO",{"v":3.0905379266008923,"d":"3.09"},{"v":3.0905379266008923,"d":"3.09"},{"v":1.371053669,"d":"1.37"}]
["08025","Crowley","CO",{"v":2.5331621512419202,"d":"2.53"},{"v":2.5331621512419202,"d":"2.53"},{"v":0.386746045,"d":"0.39"}]
["08027","Custer","CO",{"v":2.683594031905189,"d":"2.68"},{"v":2.6835940319051894,"d":"2.68"},{"v":0.757416916,"d":"0.76"}]
["08029","Delta","CO",{"v":2.8215185027422427,"d":"2.82"},{"v":2.8215185027422427,"d":"2.82"},{"v":0.805854602,"d":"0.81"}]
["08031","Denver","CO",{"v":2.4914303952100847E-6,"d":"0.00"},{"v":2.4914303952100843E-6,"d":"0.00"},{"v":3.979189888,"d":"3.98"}]
["08033","Dolores","CO",{"v":3.0027094526580895,"d":"3.00"},{"v":3.0027094526580895,"d":"3.00"},{"v":1.12120617,"d":"1.12"}]
["08035","Douglas","CO",{"v":2.5408381431215195,"d":"2.54"},{"v":2.540838143121519,"d":"2.54"},{"v":0.506826634,"d":"0.51"}]
["08037","Eagle","CO",{"v":2.859037115837534,"d":"2.86"},{"v":2.859037115837534,"d":"2.86"},{"v":0.681740327,"d":"0.68"}]
["08039","Elbert","CO",{"v":2.5819744621121354,"d":"2.58"},{"v":2.5819744621121354,"d":"2.58"},{"v":0.454821982,"d":"0.45"}]
["08041","El Paso","CO",{"v":2.4003861894305243,"d":"2.40"},{"v":2.4003861894305243,"d":"2.40"},{"v":0.300520202,"d":"0.30"}]
["08043","Fremont","CO",{"v":2.4648521725412156,"d":"2.46"},{"v":2.464852172541216,"d":"2.46"},{"v":0.383094076,"d":"0.38"}]
["08045","Garfield","CO",{"v":2.8585528471204675,"d":"2.86"},{"v":2.8585528471204675,"d":"2.86"},{"v":0.636092735,"d":"0.64"}]
["08047","Gilpin","CO",{"v":2.7600807504292835,"d":"2.76"},{"v":2.7600807504292835,"d":"2.76"},{"v":1.0210266,"d":"1.02"}]
["08049","Grand","CO",{"v":2.865202475587056,"d":"2.87"},{"v":2.865202475587056,"d":"2.87"},{"v":0.926966883,"d":"0.93"}]
["08051","Gunnison","CO",{"v":2.83065210234105,"d":"2.83"},{"v":2.8306521023410496,"d":"2.83"},{"v":0.887076437,"d":"0.89"}]
["08053","Hinsdale","CO",{"v":3.0238824482808555,"d":"3.02"},{"v":3.0238824482808555,"d":"3.02"},{"v":1.632142015,"d":"1.63"}]
["08055","Huerfano","CO",{"v":2.5757649737823867,"d":"2.58"},{"v":2.5757649737823862,"d":"2.58"},{"v":0.496406717,"d":"0.50"}]
["08057","Jackson","CO",{"v":2.943939346598164,"d":"2.94"},{"v":2.943939346598164,"d":"2.94"},{"v":0.922227144,"d":"0.92"}]
["08059","Jefferson","CO",{"v":2.317584875366952,"d":"2.32"},{"v":2.317584875366952,"d":"2.32"},{"v":0.689627284,"d":"0.69"}]
["08061","Kiowa","CO",{"v":2.5182752846754695,"d":"2.52"},{"v":2.518275284675469,"d":"2.52"},{"v":0.387141164,"d":"0.39"}]
["08063","Kit Carson","CO",{"v":2.5037970816966912,"d":"2.50"},{"v":2.5037970816966917,"d":"2.50"},{"v":0.346048558,"d":"0.35"}]
["08065","Lake","CO",{"v":2.535126377647589,"d":"2.54"},{"v":2.5351263776475887,"d":"2.54"},{"v":0.408295539,"d":"0.41"}]
["08067","La Plata","CO",{"v":2.8136298774468917,"d":"2.81"},{"v":2.813629877446892,"d":"2.81"},{"v":0.877548857,"d":"0.88"}]
["08069","Larimer","CO",{"v":2.717886005284232,"d":"2.72"},{"v":2.717886005284232,"d":"2.72"},{"v":0.507133206,"d":"0.51"}]
["08071","Las Animas","CO",{"v":2.5959143063043113,"d":"2.60"},{"v":2.595914306304311,"d":"2.60"},{"v":0.370576796,"d":"0.37"}]
["08073","Lincoln","CO",{"v":2.545846554176075,"d":"2.55"},{"v":2.5458465541760744,"d":"2.55"},{"v":0.386617017,"d":"0.39"}]
["08075","Logan","CO",{"v":2.6279563224015288,"d":"2.63"},{"v":2.6279563224015288,"d":"2.63"},{"v":0.432611149,"d":"0.43"}]
["08077","Mesa","CO",{"v":2.774594609635022,"d":"2.77"},{"v":2.774594609635022,"d":"2.77"},{"v":0.531205847,"d":"0.53"}]
["08079","Mineral","CO",{"v":3.063064879430783,"d":"3.06"},{"v":3.0630648794307826,"d":"3.06"},{"v":1.662250592,"d":"1.66"}]
["08081","Moffat","CO",{"v":2.72930618810138,"d":"2.73"},{"v":2.72930618810138,"d":"2.73"},{"v":0.509292297,"d":"0.51"}]
["08083","Montezuma","CO",{"v":2.923576571555875,"d":"2.92"},{"v":2.923576571555875,"d":"2.92"},{"v":0.842411852,"d":"0.84"}]
["08085","Montrose","CO",{"v":2.8260297104923113,"d":"2.83"},{"v":2.8260297104923118,"d":"2.83"},{"v":0.71956607,"d":"0.72"}]
["08087","Morgan","CO",{"v":2.674523287900384,"d":"2.67"},{"v":2.6745232879003837,"d":"2.67"},{"v":0.46594161,"d":"0.47"}]
["08089","Otero","CO",{"v":2.4055771019888983,"d":"2.41"},{"v":2.4055771019888983,"d":"2.41"},{"v":0.269543002,"d":"0.27"}]
["08091","Ouray","CO",{"v":2.8554040277192834,"d":"2.86"},{"v":2.855404027719283,"d":"2.86"},{"v":1.055151614,"d":"1.06"}]
["08093","Park","CO",{"v":2.8602474272872347,"d":"2.86"},{"v":2.8602474272872342,"d":"2.86"},{"v":0.809228968,"d":"0.81"}]
["08095","Phillips","CO",{"v":2.5528419221288816,"d":"2.55"},{"v":2.5528419221288816,"d":"2.55"},{"v":0.418307368,"d":"0.42"}]
["08097","Pitkin","CO",{"v":2.8878546666641456,"d":"2.89"},{"v":2.8878546666641456,"d":"2.89"},{"v":0.888779109,"d":"0.89"}]
["08099","Prowers","CO",{"v":2.426598200824364,"d":"2.43"},{"v":2.426598200824364,"d":"2.43"},{"v":0.276257233,"d":"0.28"}]
["08101","Pueblo","CO",{"v":2.406078513117599,"d":"2.41"},{"v":2.4060785131176,"d":"2.41"},{"v":0.256530402,"d":"0.26"}]
["08103","Rio Blanco","CO",{"v":2.73383171537347,"d":"2.73"},{"v":2.7338317153734697,"d":"2.73"},{"v":0.841162082,"d":"0.84"}]
["08105","Rio Grande","CO",{"v":2.8697551039956126,"d":"2.87"},{"v":2.869755103995613,"d":"2.87"},{"v":1.041039072,"d":"1.04"}]
["08107","Routt","CO",{"v":2.893797843533449,"d":"2.89"},{"v":2.893797843533449,"d":"2.89"},{"v":0.8524477830000001,"d":"0.85"}]
["08109","Saguache","CO",{"v":2.978894504462853,"d":"2.98"},{"v":2.9788945044628536,"d":"2.98"},{"v":1.259954118,"d":"1.26"}]
["08111","San Juan","CO",{"v":2.839970123560174,"d":"2.84"},{"v":2.8399701235601746,"d":"2.84"},{"v":1.225891235,"d":"1.23"}]
["08113","San Miguel","CO",{"v":2.7666109490576085,"d":"2.77"},{"v":2.7666109490576085,"d":"2.77"},{"v":0.93401411,"d":"0.93"}]
["08115","Sedgwick","CO",{"v":2.527771469430784,"d":"2.53"},{"v":2.5277714694307836,"d":"2.53"},{"v":0.417112864,"d":"0.42"}]
["08117","Summit","CO",{"v":2.842317357143197,"d":"2.84"},{"v":2.842317357143197,"d":"2.84"},{"v":0.724175546,"d":"0.72"}]
["08119","Teller","CO",{"v":2.559706046920794,"d":"2.56"},{"v":2.5597060469207937,"d":"2.56"},{"v":0.535092244,"d":"0.54"}]
["08121","Washington","CO",{"v":2.5772938516363784,"d":"2.58"},{"v":2.5772938516363784,"d":"2.58"},{"v":0.45484616,"d":"0.45"}]
["08123","Weld","CO",{"v":2.5917013788390912,"d":"2.59"},{"v":2.5917013788390912,"d":"2.59"},{"v":0.37486824,"d":"0.37"}]
["08125","Yuma","CO",{"v":2.5220255360434547,"d":"2.52"},{"v":2.5220255360434543,"d":"2.52"},{"v":0.364832621,"d":"0.36"}]
["09001","Fairfield","CT",{"v":1.0811513921778149,"d":"1.08"},{"v":1.0811513921778149,"d":"1.08"},{"v":0.928212622,"d":"0.93"}]
["09003","Hartford","CT",{"v":1.4337075715477163,"d":"1.43"},{"v":1.4337075715477163,"d":"1.43"},{"v":0.842341989,"d":"0.84"}]
["09005","Litchfield","CT",{"v":2.937292823626267,"d":"2.94"},{"v":2.9372928236262674,"d":"2.94"},{"v":1.086204539,"d":"1.09"}]
["09007","Middlesex","CT",{"v":2.616319232274477,"d":"2.62"},{"v":2.616319232274477,"d":"2.62"},{"v":0.79770281,"d":"0.80"}]
["09009","New Haven","CT",{"v":1.0392622372858942,"d":"1.04"},{"v":1.0392622372858942,"d":"1.04"},{"v":0.8806141260000001,"d":"0.88"}]
["09011","New London","CT",{"v":2.6013907803353966,"d":"2.60"},{"v":2.601390780335396,"d":"2.60"},{"v":0.769838912,"d":"0.77"}]
["09013","Tolland","CT",{"v":2.7690434085155946,"d":"2.77"},{"v":2.769043408515594,"d":"2.77"},{"v":0.9966260309999999,"d":"1.00"}]
["09015","Windham","CT",{"v":2.792249674807444,"d":"2.79"},{"v":2.7922496748074437,"d":"2.79"},{"v":0.9924175530000001,"d":"0.99"}]
["10001","Kent","DE",{"v":2.723671538230903,"d":"2.72"},{"v":2.723671538230903,"d":"2.72"},{"v":0.305779205,"d":"0.31"}]
["10003","New Castle","DE",{"v":1.6180011101090053,"d":"1.62"},{"v":1.6180011101090055,"d":"1.62"},{"v":0.490654262,"d":"0.49"}]
["10005","Sussex","DE",{"v":2.7188939673459376,"d":"2.72"},{"v":2.7188939673459376,"d":"2.72"},{"v":0.41622969,"d":"0.42"}]
["11001","District of Columbia","DC",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["12001","Alachua","FL",{"v":1.988324955290071,"d":"1.99"},{"v":1.9883249552900706,"d":"1.99"},{"v":0.169416045,"d":"0.17"}]
["12003","Baker","FL",{"v":2.0654765974082934,"d":"2.07"},{"v":2.065476597408293,"d":"2.07"},{"v":0.255417318,"d":"0.26"}]
["12005","Bay","FL",{"v":1.9016007978054428,"d":"1.90"},{"v":1.901600797805443,"d":"1.90"},{"v":0.149042943,"d":"0.15"}]
["12007","Bradford","FL",{"v":2.0738766789486784,"d":"2.07"},{"v":2.073876678948678,"d":"2.07"},{"v":0.221089708,"d":"0.22"}]
["12009","Brevard","FL",{"v":1.5758342577861844,"d":"1.58"},{"v":1.5758342577861844,"d":"1.58"},{"v":0.09725625,"d":"0.10"}]
["12011","Broward","FL",{"v":0.5882772873710899,"d":"0.59"},{"v":0.58827728737109,"d":"0.59"},{"v":0.144109188,"d":"0.14"}]
["12013","Calhoun","FL",{"v":2.0495443379329052,"d":"2.05"},{"v":2.049544337932905,"d":"2.05"},{"v":0.273880995,"d":"0.27"}]
["12015","Charlotte","FL",{"v":1.3915026653743554,"d":"1.39"},{"v":1.3915026653743554,"d":"1.39"},{"v":0.087108886,"d":"0.09"}]
["12017","Citrus","FL",{"v":1.8379819139209377,"d":"1.84"},{"v":1.8379819139209375,"d":"1.84"},{"v":0.140578395,"d":"0.14"}]
["12019","Clay","FL",{"v":1.9043041748575409,"d":"1.90"},{"v":1.904304174857541,"d":"1.90"},{"v":0.176326198,"d":"0.18"}]
["12021","Collier","FL",{"v":1.754791464871979,"d":"1.75"},{"v":1.754791464871979,"d":"1.75"},{"v":0.103526275,"d":"0.10"}]
["12023","Columbia","FL",{"v":1.9258912550498786,"d":"1.93"},{"v":1.9258912550498786,"d":"1.93"},{"v":0.23586787200000003,"d":"0.24"}]
["12027","De Soto","FL",{"v":1.9388272400447542,"d":"1.94"},{"v":1.9388272400447546,"d":"1.94"},{"v":0.14068278,"d":"0.14"}]
["12029","Dixie","FL",{"v":2.0646376359512235,"d":"2.06"},{"v":2.064637635951223,"d":"2.06"},{"v":0.227811136,"d":"0.23"}]
["12031","Duval","FL",{"v":1.1646937394381334,"d":"1.16"},{"v":1.1646937394381336,"d":"1.16"},{"v":0.212635931,"d":"0.21"}]
["12033","Escambia","FL",{"v":1.7424825514393765,"d":"1.74"},{"v":1.7424825514393767,"d":"1.74"},{"v":0.153797898,"d":"0.15"}]
["12035","Flagler","FL",{"v":1.7427936339166659,"d":"1.74"},{"v":1.7427936339166659,"d":"1.74"},{"v":0.136642559,"d":"0.14"}]
["12037","Franklin","FL",{"v":1.8295946490963202,"d":"1.83"},{"v":1.8295946490963202,"d":"1.83"},{"v":0.163210432,"d":"0.16"}]
["12039","Gadsden","FL",{"v":1.894348534152195,"d":"1.89"},{"v":1.894348534152195,"d":"1.89"},{"v":0.257953739,"d":"0.26"}]
["12041","Gilchrist","FL",{"v":1.9169724748740238,"d":"1.92"},{"v":1.916972474874024,"d":"1.92"},{"v":0.213481335,"d":"0.21"}]
["12043","Glades","FL",{"v":1.989129109061312,"d":"1.99"},{"v":1.989129109061312,"d":"1.99"},{"v":0.117869304,"d":"0.12"}]
["12045","Gulf","FL",{"v":1.8089687138693735,"d":"1.81"},{"v":1.8089687138693735,"d":"1.81"},{"v":0.199809998,"d":"0.20"}]
["12047","Hamilton","FL",{"v":1.8699568586373623,"d":"1.87"},{"v":1.8699568586373618,"d":"1.87"},{"v":0.225286405,"d":"0.23"}]
["12049","Hardee","FL",{"v":2.041849590777026,"d":"2.04"},{"v":2.041849590777026,"d":"2.04"},{"v":0.148264726,"d":"0.15"}]
["12051","Hendry","FL",{"v":1.9041429104969434,"d":"1.90"},{"v":1.9041429104969434,"d":"1.90"},{"v":0.11763847800000002,"d":"0.12"}]
["12053","Hernando","FL",{"v":1.7885396801425608,"d":"1.79"},{"v":1.788539680142561,"d":"1.79"},{"v":0.145998404,"d":"0.15"}]
["12055","Highlands","FL",{"v":1.914282520034559,"d":"1.91"},{"v":1.9142825200345592,"d":"1.91"},{"v":0.115143102,"d":"0.12"}]
["12057","Hillsborough","FL",{"v":0.9783838457090612,"d":"0.98"},{"v":0.9783838457090613,"d":"0.98"},{"v":0.1744174,"d":"0.17"}]
["12059","Holmes","FL",{"v":2.2682457486978724,"d":"2.27"},{"v":2.2682457486978724,"d":"2.27"},{"v":0.264167233,"d":"0.26"}]
["12061","Indian River","FL",{"v":1.652698466392115,"d":"1.65"},{"v":1.652698466392115,"d":"1.65"},{"v":0.108622914,"d":"0.11"}]
["12063","Jackson","FL",{"v":2.04975478976955,"d":"2.05"},{"v":2.04975478976955,"d":"2.05"},{"v":0.221451846,"d":"0.22"}]
["12065","Jefferson","FL",{"v":2.1883146572687115,"d":"2.19"},{"v":2.188314657268711,"d":"2.19"},{"v":0.290825448,"d":"0.29"}]
["12067","Lafayette","FL",{"v":2.0677707203167777,"d":"2.07"},{"v":2.0677707203167772,"d":"2.07"},{"v":0.276559897,"d":"0.28"}]
["12069","Lake","FL",{"v":1.7395785540290256,"d":"1.74"},{"v":1.7395785540290254,"d":"1.74"},{"v":0.130133529,"d":"0.13"}]
["12071","Lee","FL",{"v":1.5717217326901385,"d":"1.57"},{"v":1.5717217326901383,"d":"1.57"},{"v":0.117625058,"d":"0.12"}]
["12073","Leon","FL",{"v":1.9434013255618046,"d":"1.94"},{"v":1.9434013255618041,"d":"1.94"},{"v":0.219036291,"d":"0.22"}]
["12075","Levy","FL",{"v":2.1192115057345635,"d":"2.12"},{"v":2.119211505734564,"d":"2.12"},{"v":0.206996871,"d":"0.21"}]
["12077","Liberty","FL",{"v":2.181648359536746,"d":"2.18"},{"v":2.181648359536746,"d":"2.18"},{"v":0.351440987,"d":"0.35"}]
["12079","Madison","FL",{"v":1.8820961722696015,"d":"1.88"},{"v":1.882096172269602,"d":"1.88"},{"v":0.232988959,"d":"0.23"}]
["12081","Manatee","FL",{"v":1.76532274333672,"d":"1.77"},{"v":1.76532274333672,"d":"1.77"},{"v":0.104604294,"d":"0.10"}]
["12083","Marion","FL",{"v":1.8842253663904762,"d":"1.88"},{"v":1.884225366390476,"d":"1.88"},{"v":0.142719984,"d":"0.14"}]
["12085","Martin","FL",{"v":1.5258502347998315,"d":"1.53"},{"v":1.5258502347998317,"d":"1.53"},{"v":0.089118864,"d":"0.09"}]
["12086","Miami-Dade","FL",{"v":1.0973304075473547,"d":"1.10"},{"v":1.097330407547355,"d":"1.10"},{"v":0.133994735,"d":"0.13"}]
["12087","Monroe","FL",{"v":1.7690902081963849,"d":"1.77"},{"v":1.769090208196385,"d":"1.77"},{"v":0.070892916,"d":"0.07"}]
["12089","Nassau","FL",{"v":2.002921873754694,"d":"2.00"},{"v":2.0029218737546937,"d":"2.00"},{"v":0.189402116,"d":"0.19"}]
["12091","Okaloosa","FL",{"v":1.7710606382974912,"d":"1.77"},{"v":1.7710606382974912,"d":"1.77"},{"v":0.137379419,"d":"0.14"}]
["12093","Okeechobee","FL",{"v":1.8853177247234054,"d":"1.89"},{"v":1.8853177247234054,"d":"1.89"},{"v":0.10489006300000002,"d":"0.10"}]
["12095","Orange","FL",{"v":0.8985931184769249,"d":"0.90"},{"v":0.8985931184769249,"d":"0.90"},{"v":0.196287338,"d":"0.20"}]
["12097","Osceola","FL",{"v":1.6465788280356146,"d":"1.65"},{"v":1.6465788280356146,"d":"1.65"},{"v":0.095833366,"d":"0.10"}]
["12099","Palm Beach","FL",{"v":1.5027623209555157,"d":"1.50"},{"v":1.5027623209555154,"d":"1.50"},{"v":0.092783226,"d":"0.09"}]
["12101","Pasco","FL",{"v":1.7430009672741713,"d":"1.74"},{"v":1.7430009672741713,"d":"1.74"},{"v":0.153540929,"d":"0.15"}]
["12103","Pinellas","FL",{"v":9.1581320198943318E-5,"d":"0.00"},{"v":9.15813201989433e-05,"d":"0.00"},{"v":0.442017252,"d":"0.44"}]
["12105","Polk","FL",{"v":1.8470746680479202,"d":"1.85"},{"v":1.8470746680479202,"d":"1.85"},{"v":0.126327251,"d":"0.13"}]
["12107","Putnam","FL",{"v":1.8763836078056273,"d":"1.88"},{"v":1.8763836078056273,"d":"1.88"},{"v":0.19115332199999996,"d":"0.19"}]
["12109","St Johns","FL",{"v":1.8821099398666281,"d":"1.88"},{"v":1.8821099398666283,"d":"1.88"},{"v":0.156223052,"d":"0.16"}]
["12111","St Lucie","FL",{"v":1.612537719233661,"d":"1.61"},{"v":1.612537719233661,"d":"1.61"},{"v":0.11949603500000001,"d":"0.12"}]
["12113","Santa Rosa","FL",{"v":2.0620711492965196,"d":"2.06"},{"v":2.0620711492965196,"d":"2.06"},{"v":0.163121051,"d":"0.16"}]
["12115","Sarasota","FL",{"v":1.7844529610349087,"d":"1.78"},{"v":1.7844529610349087,"d":"1.78"},{"v":0.11454346899999998,"d":"0.11"}]
["12117","Seminole","FL",{"v":0.8559218769713611,"d":"0.86"},{"v":0.855921876971361,"d":"0.86"},{"v":0.21349032,"d":"0.21"}]
["12119","Sumter","FL",{"v":1.897273159593711,"d":"1.90"},{"v":1.8972731595937107,"d":"1.90"},{"v":0.117529281,"d":"0.12"}]
["12121","Suwannee","FL",{"v":2.208140593817839,"d":"2.21"},{"v":2.208140593817839,"d":"2.21"},{"v":0.20846755,"d":"0.21"}]
["12123","Taylor","FL",{"v":2.0231089345550983,"d":"2.02"},{"v":2.0231089345550983,"d":"2.02"},{"v":0.19307269799999996,"d":"0.19"}]
["12125","Union","FL",{"v":1.9409272676980813,"d":"1.94"},{"v":1.940927267698081,"d":"1.94"},{"v":0.251182696,"d":"0.25"}]
["12127","Volusia","FL",{"v":1.6704653449855404,"d":"1.67"},{"v":1.6704653449855407,"d":"1.67"},{"v":0.129781549,"d":"0.13"}]
["12129","Wakulla","FL",{"v":2.1426528305452495,"d":"2.14"},{"v":2.1426528305452495,"d":"2.14"},{"v":0.260153131,"d":"0.26"}]
["12131","Walton","FL",{"v":2.010331399613907,"d":"2.01"},{"v":2.010331399613907,"d":"2.01"},{"v":0.195607902,"d":"0.20"}]
["12133","Washington","FL",{"v":2.0444835690749437,"d":"2.04"},{"v":2.044483569074944,"d":"2.04"},{"v":0.257827489,"d":"0.26"}]
["13001","Appling","GA",{"v":1.7765432445103184,"d":"1.78"},{"v":1.7765432445103182,"d":"1.78"},{"v":0.21638796999999999,"d":"0.22"}]
["13003","Atkinson","GA",{"v":1.819377528488493,"d":"1.82"},{"v":1.8193775284884932,"d":"1.82"},{"v":0.27084273,"d":"0.27"}]
["13005","Bacon","GA",{"v":2.024487873203122,"d":"2.02"},{"v":2.024487873203122,"d":"2.02"},{"v":0.196956827,"d":"0.20"}]
["13007","Baker","GA",{"v":1.8955748754103612,"d":"1.90"},{"v":1.8955748754103612,"d":"1.90"},{"v":0.207059672,"d":"0.21"}]
["13009","Baldwin","GA",{"v":1.634604124917838,"d":"1.63"},{"v":1.634604124917838,"d":"1.63"},{"v":0.254635189,"d":"0.25"}]
["13011","Banks","GA",{"v":1.7235013585458634,"d":"1.72"},{"v":1.7235013585458632,"d":"1.72"},{"v":0.366837999,"d":"0.37"}]
["13013","Barrow","GA",{"v":1.7942456340471074,"d":"1.79"},{"v":1.7942456340471071,"d":"1.79"},{"v":0.299484487,"d":"0.30"}]
["13015","Bartow","GA",{"v":1.886326214133797,"d":"1.89"},{"v":1.886326214133797,"d":"1.89"},{"v":0.279617796,"d":"0.28"}]
["13017","Ben Hill","GA",{"v":1.6797442111412235,"d":"1.68"},{"v":1.6797442111412237,"d":"1.68"},{"v":0.186654495,"d":"0.19"}]
["13019","Berrien","GA",{"v":1.7822116183425085,"d":"1.78"},{"v":1.782211618342508,"d":"1.78"},{"v":0.233567012,"d":"0.23"}]
["13021","Bibb","GA",{"v":1.4410654672809893,"d":"1.44"},{"v":1.441065467280989,"d":"1.44"},{"v":0.21408867800000003,"d":"0.21"}]
["13023","Bleckley","GA",{"v":1.8402153346629444,"d":"1.84"},{"v":1.8402153346629444,"d":"1.84"},{"v":0.218318949,"d":"0.22"}]
["13025","Brantley","GA",{"v":1.9005250454453162,"d":"1.90"},{"v":1.9005250454453162,"d":"1.90"},{"v":0.28423272,"d":"0.28"}]
["13027","Brooks","GA",{"v":1.7866893640469006,"d":"1.79"},{"v":1.7866893640469006,"d":"1.79"},{"v":0.20313238900000002,"d":"0.20"}]
["13029","Bryan","GA",{"v":1.8435569934167195,"d":"1.84"},{"v":1.8435569934167195,"d":"1.84"},{"v":0.217258301,"d":"0.22"}]
["13031","Bulloch","GA",{"v":1.6310533545119072,"d":"1.63"},{"v":1.6310533545119072,"d":"1.63"},{"v":0.224031531,"d":"0.22"}]
["13033","Burke","GA",{"v":1.7876385122689185,"d":"1.79"},{"v":1.7876385122689182,"d":"1.79"},{"v":0.235593533,"d":"0.24"}]
["13035","Butts","GA",{"v":1.9396077841929653,"d":"1.94"},{"v":1.939607784192965,"d":"1.94"},{"v":0.290056454,"d":"0.29"}]
["13037","Calhoun","GA",{"v":1.6403592387819963,"d":"1.64"},{"v":1.6403592387819963,"d":"1.64"},{"v":0.219633711,"d":"0.22"}]
["13039","Camden","GA",{"v":1.7275183137403427,"d":"1.73"},{"v":1.7275183137403427,"d":"1.73"},{"v":0.164696507,"d":"0.16"}]
["13043","Candler","GA",{"v":1.7548095868169795,"d":"1.75"},{"v":1.7548095868169793,"d":"1.75"},{"v":0.234873351,"d":"0.23"}]
["13045","Carroll","GA",{"v":1.8213064057137427,"d":"1.82"},{"v":1.8213064057137427,"d":"1.82"},{"v":0.242700775,"d":"0.24"}]
["13047","Catoosa","GA",{"v":2.119615943998845,"d":"2.12"},{"v":2.119615943998845,"d":"2.12"},{"v":0.303017845,"d":"0.30"}]
["13049","Charlton","GA",{"v":1.8764320686191658,"d":"1.88"},{"v":1.8764320686191656,"d":"1.88"},{"v":0.251220394,"d":"0.25"}]
["13051","Chatham","GA",{"v":1.493915139431025,"d":"1.49"},{"v":1.493915139431025,"d":"1.49"},{"v":0.112750657,"d":"0.11"}]
["13053","Chattahoochee","GA",{"v":1.779599714194248,"d":"1.78"},{"v":1.779599714194248,"d":"1.78"},{"v":0.25819529,"d":"0.26"}]
["13055","Chattooga","GA",{"v":1.901736258657963,"d":"1.90"},{"v":1.9017362586579625,"d":"1.90"},{"v":0.340702532,"d":"0.34"}]
["13057","Cherokee","GA",{"v":1.4652353717204527,"d":"1.47"},{"v":1.465235371720453,"d":"1.47"},{"v":0.262535548,"d":"0.26"}]
["13059","Clarke","GA",{"v":1.221815717440484,"d":"1.22"},{"v":1.221815717440484,"d":"1.22"},{"v":0.352882935,"d":"0.35"}]
["13061","Clay","GA",{"v":1.8658074878760982,"d":"1.87"},{"v":1.8658074878760984,"d":"1.87"},{"v":0.237276963,"d":"0.24"}]
["13063","Clayton","GA",{"v":0.3099645313114723,"d":"0.31"},{"v":0.3099645313114723,"d":"0.31"},{"v":0.355762955,"d":"0.36"}]
["13065","Clinch","GA",{"v":1.7128190494083988,"d":"1.71"},{"v":1.7128190494083988,"d":"1.71"},{"v":0.252840247,"d":"0.25"}]
["13067","Cobb","GA",{"v":0.0694765209092933,"d":"0.07"},{"v":0.0694765209092933,"d":"0.07"},{"v":0.468832126,"d":"0.47"}]
["13069","Coffee","GA",{"v":1.6715982409650452,"d":"1.67"},{"v":1.6715982409650454,"d":"1.67"},{"v":0.214894568,"d":"0.21"}]
["13071","Colquitt","GA",{"v":1.7623728518372876,"d":"1.76"},{"v":1.7623728518372876,"d":"1.76"},{"v":0.192772981,"d":"0.19"}]
["13073","Columbia","GA",{"v":1.549447973601518,"d":"1.55"},{"v":1.549447973601518,"d":"1.55"},{"v":0.198474829,"d":"0.20"}]
["13075","Cook","GA",{"v":1.717290999918047,"d":"1.72"},{"v":1.717290999918047,"d":"1.72"},{"v":0.197973207,"d":"0.20"}]
["13077","Coweta","GA",{"v":1.444774972199746,"d":"1.44"},{"v":1.444774972199746,"d":"1.44"},{"v":0.225669321,"d":"0.23"}]
["13079","Crawford","GA",{"v":1.7968872652663352,"d":"1.80"},{"v":1.796887265266335,"d":"1.80"},{"v":0.307893442,"d":"0.31"}]
["13081","Crisp","GA",{"v":1.9448220783349708,"d":"1.94"},{"v":1.9448220783349708,"d":"1.94"},{"v":0.17457865500000003,"d":"0.17"}]
["13083","Dade","GA",{"v":1.7981461959281748,"d":"1.80"},{"v":1.7981461959281748,"d":"1.80"},{"v":0.411249858,"d":"0.41"}]
["13085","Dawson","GA",{"v":1.9385509083806534,"d":"1.94"},{"v":1.9385509083806538,"d":"1.94"},{"v":0.430176168,"d":"0.43"}]
["13087","Decatur","GA",{"v":1.833402195230476,"d":"1.83"},{"v":1.8334021952304762,"d":"1.83"},{"v":0.187004947,"d":"0.19"}]
["13089","De Kalb","GA",{"v":0.008573336133457326,"d":"0.01"},{"v":0.008573336133457326,"d":"0.01"},{"v":0.706325967,"d":"0.71"}]
["13091","Dodge","GA",{"v":1.7591666930091754,"d":"1.76"},{"v":1.759166693009175,"d":"1.76"},{"v":0.255125007,"d":"0.26"}]
["13093","Dooly","GA",{"v":1.8240031490004704,"d":"1.82"},{"v":1.8240031490004707,"d":"1.82"},{"v":0.175309024,"d":"0.18"}]
["13095","Dougherty","GA",{"v":1.7687093016605067,"d":"1.77"},{"v":1.7687093016605069,"d":"1.77"},{"v":0.181386122,"d":"0.18"}]
["13097","Douglas","GA",{"v":1.4026873949087786,"d":"1.40"},{"v":1.4026873949087786,"d":"1.40"},{"v":0.237590326,"d":"0.24"}]
["13099","Early","GA",{"v":1.7433234387600478,"d":"1.74"},{"v":1.7433234387600476,"d":"1.74"},{"v":0.189923666,"d":"0.19"}]
["13101","Echols","GA",{"v":1.8878281813976925,"d":"1.89"},{"v":1.8878281813976925,"d":"1.89"},{"v":0.320339902,"d":"0.32"}]
["13103","Effingham","GA",{"v":1.9136224141957396,"d":"1.91"},{"v":1.9136224141957396,"d":"1.91"},{"v":0.287868954,"d":"0.29"}]
["13105","Elbert","GA",{"v":1.7115333350180912,"d":"1.71"},{"v":1.7115333350180915,"d":"1.71"},{"v":0.266760587,"d":"0.27"}]
["13107","Emanuel","GA",{"v":1.613392770447178,"d":"1.61"},{"v":1.6133927704471782,"d":"1.61"},{"v":0.24518141699999998,"d":"0.25"}]
["13109","Evans","GA",{"v":1.5635117076689253,"d":"1.56"},{"v":1.5635117076689253,"d":"1.56"},{"v":0.209244746,"d":"0.21"}]
["13111","Fannin","GA",{"v":1.9814033057192444,"d":"1.98"},{"v":1.9814033057192442,"d":"1.98"},{"v":0.540690543,"d":"0.54"}]
["13113","Fayette","GA",{"v":1.4807513098284426,"d":"1.48"},{"v":1.4807513098284426,"d":"1.48"},{"v":0.202208023,"d":"0.20"}]
["13115","Floyd","GA",{"v":1.7717234180981105,"d":"1.77"},{"v":1.77172341809811,"d":"1.77"},{"v":0.257859016,"d":"0.26"}]
["13117","Forsyth","GA",{"v":1.4650757381449306,"d":"1.47"},{"v":1.4650757381449306,"d":"1.47"},{"v":0.23756744,"d":"0.24"}]
["13119","Franklin","GA",{"v":1.9910731734402645,"d":"1.99"},{"v":1.9910731734402645,"d":"1.99"},{"v":0.303352782,"d":"0.30"}]
["13121","Fulton","GA",{"v":0.14072669347752448,"d":"0.14"},{"v":0.14072669347752448,"d":"0.14"},{"v":0.471987782,"d":"0.47"}]
["13123","Gilmer","GA",{"v":1.9521033416559395,"d":"1.95"},{"v":1.9521033416559397,"d":"1.95"},{"v":0.52759857,"d":"0.53"}]
["13125","Glascock","GA",{"v":1.8989123152376037,"d":"1.90"},{"v":1.8989123152376035,"d":"1.90"},{"v":0.287024575,"d":"0.29"}]
["13127","Glynn","GA",{"v":1.6159656843507293,"d":"1.62"},{"v":1.6159656843507293,"d":"1.62"},{"v":0.129883548,"d":"0.13"}]
["13129","Gordon","GA",{"v":1.858079463469203,"d":"1.86"},{"v":1.8580794634692026,"d":"1.86"},{"v":0.305588955,"d":"0.31"}]
["13131","Grady","GA",{"v":1.8519100266418882,"d":"1.85"},{"v":1.8519100266418878,"d":"1.85"},{"v":0.207627779,"d":"0.21"}]
["13133","Greene","GA",{"v":1.6865161118995466,"d":"1.69"},{"v":1.6865161118995466,"d":"1.69"},{"v":0.297824292,"d":"0.30"}]
["13135","Gwinnett","GA",{"v":0.28540681385265254,"d":"0.29"},{"v":0.28540681385265254,"d":"0.29"},{"v":0.420559873,"d":"0.42"}]
["13137","Habersham","GA",{"v":1.8690257912553767,"d":"1.87"},{"v":1.869025791255377,"d":"1.87"},{"v":0.37051251,"d":"0.37"}]
["13139","Hall","GA",{"v":1.6306527174971361,"d":"1.63"},{"v":1.630652717497136,"d":"1.63"},{"v":0.271776314,"d":"0.27"}]
["13141","Hancock","GA",{"v":1.925256225897319,"d":"1.93"},{"v":1.925256225897319,"d":"1.93"},{"v":0.302847663,"d":"0.30"}]
["13143","Haralson","GA",{"v":1.7277543160654845,"d":"1.73"},{"v":1.7277543160654842,"d":"1.73"},{"v":0.31465115,"d":"0.31"}]
["13145","Harris","GA",{"v":1.6613228676539573,"d":"1.66"},{"v":1.6613228676539573,"d":"1.66"},{"v":0.359308676,"d":"0.36"}]
["13147","Hart","GA",{"v":1.9124529697416468,"d":"1.91"},{"v":1.9124529697416468,"d":"1.91"},{"v":0.239886638,"d":"0.24"}]
["13149","Heard","GA",{"v":1.735057805293797,"d":"1.74"},{"v":1.7350578052937973,"d":"1.74"},{"v":0.354621862,"d":"0.35"}]
["13151","Henry","GA",{"v":1.5403307118672867,"d":"1.54"},{"v":1.5403307118672864,"d":"1.54"},{"v":0.202425754,"d":"0.20"}]
["13153","Houston","GA",{"v":1.7875203557089194,"d":"1.79"},{"v":1.7875203557089194,"d":"1.79"},{"v":0.213348127,"d":"0.21"}]
["13155","Irwin","GA",{"v":1.7993540388253533,"d":"1.80"},{"v":1.7993540388253537,"d":"1.80"},{"v":0.195991857,"d":"0.20"}]
["13157","Jackson","GA",{"v":1.9463129695801535,"d":"1.95"},{"v":1.9463129695801535,"d":"1.95"},{"v":0.315294627,"d":"0.32"}]
["13159","Jasper","GA",{"v":1.7944813445428203,"d":"1.79"},{"v":1.79448134454282,"d":"1.79"},{"v":0.308465612,"d":"0.31"}]
["13161","Jeff Davis","GA",{"v":2.0023791542962623,"d":"2.00"},{"v":2.0023791542962623,"d":"2.00"},{"v":0.228053807,"d":"0.23"}]
["13163","Jefferson","GA",{"v":1.8572528371135402,"d":"1.86"},{"v":1.8572528371135402,"d":"1.86"},{"v":0.237048077,"d":"0.24"}]
["13165","Jenkins","GA",{"v":1.7481917321884575,"d":"1.75"},{"v":1.748191732188457,"d":"1.75"},{"v":0.22567683,"d":"0.23"}]
["13167","Johnson","GA",{"v":1.7801971757508996,"d":"1.78"},{"v":1.7801971757508996,"d":"1.78"},{"v":0.262918283,"d":"0.26"}]
["13169","Jones","GA",{"v":1.7098430762354702,"d":"1.71"},{"v":1.7098430762354704,"d":"1.71"},{"v":0.286003621,"d":"0.29"}]
["13171","Lamar","GA",{"v":1.9256937593442176,"d":"1.93"},{"v":1.9256937593442176,"d":"1.93"},{"v":0.26949487,"d":"0.27"}]
["13173","Lanier","GA",{"v":1.713229097698288,"d":"1.71"},{"v":1.7132290976982878,"d":"1.71"},{"v":0.257269707,"d":"0.26"}]
["13175","Laurens","GA",{"v":1.7583400675320582,"d":"1.76"},{"v":1.758340067532058,"d":"1.76"},{"v":0.256699751,"d":"0.26"}]
["13177","Lee","GA",{"v":1.8087077152897246,"d":"1.81"},{"v":1.8087077152897246,"d":"1.81"},{"v":0.184160153,"d":"0.18"}]
["13179","Liberty","GA",{"v":1.6342582982397285,"d":"1.63"},{"v":1.6342582982397282,"d":"1.63"},{"v":0.181118109,"d":"0.18"}]
["13181","Lincoln","GA",{"v":1.9130992378854181,"d":"1.91"},{"v":1.9130992378854184,"d":"1.91"},{"v":0.344720729,"d":"0.34"}]
["13183","Long","GA",{"v":1.881014901987625,"d":"1.88"},{"v":1.8810149019876257,"d":"1.88"},{"v":0.279754644,"d":"0.28"}]
["13185","Lowndes","GA",{"v":1.6707618362907217,"d":"1.67"},{"v":1.6707618362907215,"d":"1.67"},{"v":0.20294613,"d":"0.20"}]
["13187","Lumpkin","GA",{"v":2.080121502578673,"d":"2.08"},{"v":2.0801215025786735,"d":"2.08"},{"v":0.507381347,"d":"0.51"}]
["13189","McDuffie","GA",{"v":1.5589217720829351,"d":"1.56"},{"v":1.5589217720829351,"d":"1.56"},{"v":0.233926309,"d":"0.23"}]
["13191","McIntosh","GA",{"v":1.710042317736638,"d":"1.71"},{"v":1.710042317736638,"d":"1.71"},{"v":0.171156451,"d":"0.17"}]
["13193","Macon","GA",{"v":1.9651870057372796,"d":"1.97"},{"v":1.9651870057372793,"d":"1.97"},{"v":0.256204339,"d":"0.26"}]
["13195","Madison","GA",{"v":1.6937522985056952,"d":"1.69"},{"v":1.6937522985056952,"d":"1.69"},{"v":0.319037077,"d":"0.32"}]
["13197","Marion","GA",{"v":1.9084799382046889,"d":"1.91"},{"v":1.9084799382046889,"d":"1.91"},{"v":0.319738203,"d":"0.32"}]
["13199","Meriwether","GA",{"v":1.8157486867322619,"d":"1.82"},{"v":1.815748686732262,"d":"1.82"},{"v":0.328994473,"d":"0.33"}]
["13201","Miller","GA",{"v":1.6062050342097924,"d":"1.61"},{"v":1.6062050342097924,"d":"1.61"},{"v":0.174655461,"d":"0.17"}]
["13205","Mitchell","GA",{"v":1.6044330130848252,"d":"1.60"},{"v":1.6044330130848252,"d":"1.60"},{"v":0.185563275,"d":"0.19"}]
["13207","Monroe","GA",{"v":1.9081222263812014,"d":"1.91"},{"v":1.9081222263812014,"d":"1.91"},{"v":0.291705311,"d":"0.29"}]
["13209","Montgomery","GA",{"v":1.8615936375933972,"d":"1.86"},{"v":1.8615936375933972,"d":"1.86"},{"v":0.299144192,"d":"0.30"}]
["13211","Morgan","GA",{"v":1.6394016309718307,"d":"1.64"},{"v":1.6394016309718307,"d":"1.64"},{"v":0.257303601,"d":"0.26"}]
["13213","Murray","GA",{"v":2.139236981270518,"d":"2.14"},{"v":2.139236981270518,"d":"2.14"},{"v":0.421588605,"d":"0.42"}]
["13215","Muscogee","GA",{"v":1.4124115014119631,"d":"1.41"},{"v":1.4124115014119631,"d":"1.41"},{"v":0.235014098,"d":"0.24"}]
["13217","Newton","GA",{"v":1.6477019065570062,"d":"1.65"},{"v":1.6477019065570064,"d":"1.65"},{"v":0.22049374899999996,"d":"0.22"}]
["13219","Oconee","GA",{"v":1.7876664658513728,"d":"1.79"},{"v":1.787666465851373,"d":"1.79"},{"v":0.295038469,"d":"0.30"}]
["13221","Oglethorpe","GA",{"v":1.888979740897041,"d":"1.89"},{"v":1.8889797408970412,"d":"1.89"},{"v":0.385860022,"d":"0.39"}]
["13223","Paulding","GA",{"v":1.802985205691018,"d":"1.80"},{"v":1.802985205691018,"d":"1.80"},{"v":0.273273628,"d":"0.27"}]
["13225","Peach","GA",{"v":1.3710505294126418,"d":"1.37"},{"v":1.3710505294126418,"d":"1.37"},{"v":0.210296113,"d":"0.21"}]
["13227","Pickens","GA",{"v":1.6912898175986397,"d":"1.69"},{"v":1.6912898175986395,"d":"1.69"},{"v":0.420615086,"d":"0.42"}]
["13229","Pierce","GA",{"v":1.7405317265497997,"d":"1.74"},{"v":1.7405317265498,"d":"1.74"},{"v":0.222380598,"d":"0.22"}]
["13231","Pike","GA",{"v":1.8728132344410637,"d":"1.87"},{"v":1.8728132344410635,"d":"1.87"},{"v":0.31692638,"d":"0.32"}]
["13233","Polk","GA",{"v":1.8777288388755198,"d":"1.88"},{"v":1.8777288388755198,"d":"1.88"},{"v":0.296704735,"d":"0.30"}]
["13235","Pulaski","GA",{"v":1.849509867098761,"d":"1.85"},{"v":1.8495098670987613,"d":"1.85"},{"v":0.208370599,"d":"0.21"}]
["13237","Putnam","GA",{"v":1.853926870534281,"d":"1.85"},{"v":1.8539268705342813,"d":"1.85"},{"v":0.300598566,"d":"0.30"}]
["13239","Quitman","GA",{"v":2.1471759555087475,"d":"2.15"},{"v":2.147175955508748,"d":"2.15"},{"v":0.258140408,"d":"0.26"}]
["13241","Rabun","GA",{"v":1.956676573023316,"d":"1.96"},{"v":1.956676573023316,"d":"1.96"},{"v":0.483930179,"d":"0.48"}]
["13243","Randolph","GA",{"v":1.7327999297793557,"d":"1.73"},{"v":1.732799929779356,"d":"1.73"},{"v":0.20051320000000003,"d":"0.20"}]
["13245","Richmond","GA",{"v":1.447826836003102,"d":"1.45"},{"v":1.447826836003102,"d":"1.45"},{"v":0.179519614,"d":"0.18"}]
["13247","Rockdale","GA",{"v":1.3986135955059245,"d":"1.40"},{"v":1.3986135955059245,"d":"1.40"},{"v":0.19737960100000002,"d":"0.20"}]
["13249","Schley","GA",{"v":1.941297868534823,"d":"1.94"},{"v":1.9412978685348228,"d":"1.94"},{"v":0.332510076,"d":"0.33"}]
["13251","Screven","GA",{"v":1.7563738292217013,"d":"1.76"},{"v":1.756373829221701,"d":"1.76"},{"v":0.256747857,"d":"0.26"}]
["13253","Seminole","GA",{"v":1.8991667743007152,"d":"1.90"},{"v":1.899166774300715,"d":"1.90"},{"v":0.164526564,"d":"0.16"}]
["13255","Spalding","GA",{"v":1.5038694021559131,"d":"1.50"},{"v":1.503869402155913,"d":"1.50"},{"v":0.231990042,"d":"0.23"}]
["13257","Stephens","GA",{"v":1.918444362634065,"d":"1.92"},{"v":1.9184443626340653,"d":"1.92"},{"v":0.325123899,"d":"0.33"}]
["13259","Stewart","GA",{"v":1.833629437726539,"d":"1.83"},{"v":1.8336294377265392,"d":"1.83"},{"v":0.28272346,"d":"0.28"}]
["13261","Sumter","GA",{"v":1.6359463074865788,"d":"1.64"},{"v":1.6359463074865788,"d":"1.64"},{"v":0.177584686,"d":"0.18"}]
["13263","Talbot","GA",{"v":1.8400742721930314,"d":"1.84"},{"v":1.8400742721930317,"d":"1.84"},{"v":0.365033152,"d":"0.37"}]
["13265","Taliaferro","GA",{"v":1.8279672117350085,"d":"1.83"},{"v":1.8279672117350088,"d":"1.83"},{"v":0.340352297,"d":"0.34"}]
["13267","Tattnall","GA",{"v":1.6276724888155087,"d":"1.63"},{"v":1.6276724888155087,"d":"1.63"},{"v":0.21515902,"d":"0.22"}]
["13269","Taylor","GA",{"v":1.8793835781584254,"d":"1.88"},{"v":1.8793835781584252,"d":"1.88"},{"v":0.300179634,"d":"0.30"}]
["13271","Telfair","GA",{"v":1.754186550155206,"d":"1.75"},{"v":1.754186550155206,"d":"1.75"},{"v":0.239893263,"d":"0.24"}]
["13273","Terrell","GA",{"v":1.609710792451161,"d":"1.61"},{"v":1.609710792451161,"d":"1.61"},{"v":0.18395148399999997,"d":"0.18"}]
["13275","Thomas","GA",{"v":1.7463497093003708,"d":"1.75"},{"v":1.7463497093003708,"d":"1.75"},{"v":0.192928886,"d":"0.19"}]
["13277","Tift","GA",{"v":1.5671657383029909,"d":"1.57"},{"v":1.5671657383029909,"d":"1.57"},{"v":0.174739241,"d":"0.17"}]
["13279","Toombs","GA",{"v":1.6162068943060532,"d":"1.62"},{"v":1.6162068943060532,"d":"1.62"},{"v":0.193223304,"d":"0.19"}]
["13281","Towns","GA",{"v":1.6874554849004344,"d":"1.69"},{"v":1.6874554849004346,"d":"1.69"},{"v":0.534570758,"d":"0.53"}]
["13283","Treutlen","GA",{"v":1.9011279879105158,"d":"1.90"},{"v":1.9011279879105158,"d":"1.90"},{"v":0.267889248,"d":"0.27"}]
["13285","Troup","GA",{"v":1.6410141237334424,"d":"1.64"},{"v":1.6410141237334424,"d":"1.64"},{"v":0.255717595,"d":"0.26"}]
["13287","Turner","GA",{"v":1.7821824284988528,"d":"1.78"},{"v":1.7821824284988528,"d":"1.78"},{"v":0.16868225000000003,"d":"0.17"}]
["13289","Twiggs","GA",{"v":1.972803303642588,"d":"1.97"},{"v":1.9728033036425878,"d":"1.97"},{"v":0.323010414,"d":"0.32"}]
["13291","Union","GA",{"v":2.036172129547157,"d":"2.04"},{"v":2.036172129547157,"d":"2.04"},{"v":0.522763215,"d":"0.52"}]
["13293","Upson","GA",{"v":1.7300125171051524,"d":"1.73"},{"v":1.7300125171051521,"d":"1.73"},{"v":0.253136856,"d":"0.25"}]
["13295","Walker","GA",{"v":1.6313505010996843,"d":"1.63"},{"v":1.631350501099684,"d":"1.63"},{"v":0.341158133,"d":"0.34"}]
["13297","Walton","GA",{"v":1.5646694628753375,"d":"1.56"},{"v":1.5646694628753373,"d":"1.56"},{"v":0.288579849,"d":"0.29"}]
["13299","Ware","GA",{"v":1.6974250317886337,"d":"1.70"},{"v":1.6974250317886335,"d":"1.70"},{"v":0.192144103,"d":"0.19"}]
["13301","Warren","GA",{"v":1.7157429397237902,"d":"1.72"},{"v":1.7157429397237902,"d":"1.72"},{"v":0.296681593,"d":"0.30"}]
["13303","Washington","GA",{"v":1.8641293020457634,"d":"1.86"},{"v":1.8641293020457639,"d":"1.86"},{"v":0.255707305,"d":"0.26"}]
["13305","Wayne","GA",{"v":1.769794694582959,"d":"1.77"},{"v":1.7697946945829592,"d":"1.77"},{"v":0.23064182700000002,"d":"0.23"}]
["13307","Webster","GA",{"v":1.9107710801706002,"d":"1.91"},{"v":1.9107710801706002,"d":"1.91"},{"v":0.263087319,"d":"0.26"}]
["13309","Wheeler","GA",{"v":1.9140113298573984,"d":"1.91"},{"v":1.914011329857398,"d":"1.91"},{"v":0.31671261,"d":"0.32"}]
["13311","White","GA",{"v":1.982076345077715,"d":"1.98"},{"v":1.9820763450777148,"d":"1.98"},{"v":0.47532946,"d":"0.48"}]
["13313","Whitfield","GA",{"v":1.9294362778969947,"d":"1.93"},{"v":1.9294362778969947,"d":"1.93"},{"v":0.342428125,"d":"0.34"}]
["13315","Wilcox","GA",{"v":1.8901641497715596,"d":"1.89"},{"v":1.8901641497715593,"d":"1.89"},{"v":0.241030373,"d":"0.24"}]
["13317","Wilkes","GA",{"v":1.8069708743779518,"d":"1.81"},{"v":1.8069708743779516,"d":"1.81"},{"v":0.310780819,"d":"0.31"}]
["13319","Wilkinson","GA",{"v":1.8686126326783654,"d":"1.87"},{"v":1.8686126326783652,"d":"1.87"},{"v":0.319724684,"d":"0.32"}]
["13321","Worth","GA",{"v":1.756080237278586,"d":"1.76"},{"v":1.7560802372785862,"d":"1.76"},{"v":0.201721912,"d":"0.20"}]
["15001","Hawaii","HI",{"v":0.6275886444773129,"d":"0.63"},{"v":0.6275886444773128,"d":"0.63"},{"v":0.043837752,"d":"0.04"}]
["15003","Honolulu","HI",{"v":0.2881692109882948,"d":"0.29"},{"v":0.2881692109882948,"d":"0.29"},{"v":0.081825794,"d":"0.08"}]
["15005","Kalawao","HI",{"v":0.6274326879132682,"d":"0.63"},{"v":0.6274326879132684,"d":"0.63"},{"v":0.050895221,"d":"0.05"}]
["15007","Kauai","HI",{"v":0.6195254861293361,"d":"0.62"},{"v":0.6195254861293361,"d":"0.62"},{"v":0.038649904,"d":"0.04"}]
["15009","Maui","HI",{"v":0.6231280820645599,"d":"0.62"},{"v":0.6231280820645598,"d":"0.62"},{"v":0.039799865,"d":"0.04"}]
["16001","Ada","ID",{"v":2.0226491007468064,"d":"2.02"},{"v":2.0226491007468064,"d":"2.02"},{"v":0.233392849,"d":"0.23"}]
["16003","Adams","ID",{"v":2.6807481159069195,"d":"2.68"},{"v":2.680748115906919,"d":"2.68"},{"v":1.487631972,"d":"1.49"}]
["16005","Bannock","ID",{"v":2.3623897642598104,"d":"2.36"},{"v":2.3623897642598095,"d":"2.36"},{"v":0.517815803,"d":"0.52"}]
["16007","Bear Lake","ID",{"v":2.5149545467660017,"d":"2.51"},{"v":2.5149545467660017,"d":"2.51"},{"v":0.8337939,"d":"0.83"}]
["16009","Benewah","ID",{"v":2.5950249535266168,"d":"2.60"},{"v":2.5950249535266168,"d":"2.60"},{"v":1.252015739,"d":"1.25"}]
["16011","Bingham","ID",{"v":2.4394430207405633,"d":"2.44"},{"v":2.4394430207405633,"d":"2.44"},{"v":0.592990501,"d":"0.59"}]
["16013","Blaine","ID",{"v":2.1642845067680545,"d":"2.16"},{"v":2.1642845067680545,"d":"2.16"},{"v":0.381478442,"d":"0.38"}]
["16015","Boise","ID",{"v":2.6733128806330133,"d":"2.67"},{"v":2.6733128806330133,"d":"2.67"},{"v":1.448932309,"d":"1.45"}]
["16017","Bonner","ID",{"v":2.6162662732664357,"d":"2.62"},{"v":2.6162662732664357,"d":"2.62"},{"v":1.308291226,"d":"1.31"}]
["16019","Bonneville","ID",{"v":2.448146504887669,"d":"2.45"},{"v":2.448146504887669,"d":"2.45"},{"v":0.545969561,"d":"0.55"}]
["16021","Boundary","ID",{"v":2.5789913515693845,"d":"2.58"},{"v":2.578991351569385,"d":"2.58"},{"v":1.316749729,"d":"1.32"}]
["16023","Butte","ID",{"v":2.484360528999004,"d":"2.48"},{"v":2.4843605289990043,"d":"2.48"},{"v":0.862633021,"d":"0.86"}]
["16025","Camas","ID",{"v":2.6281822109902526,"d":"2.63"},{"v":2.628182210990252,"d":"2.63"},{"v":1.215641041,"d":"1.22"}]
["16027","Canyon","ID",{"v":2.11642719212061,"d":"2.12"},{"v":2.11642719212061,"d":"2.12"},{"v":0.290188107,"d":"0.29"}]
["16029","Caribou","ID",{"v":2.4248120974871656,"d":"2.42"},{"v":2.424812097487166,"d":"2.42"},{"v":0.6604468830000001,"d":"0.66"}]
["16031","Cassia","ID",{"v":2.474118151357597,"d":"2.47"},{"v":2.474118151357597,"d":"2.47"},{"v":0.699835241,"d":"0.70"}]
["16033","Clark","ID",{"v":2.528076357698092,"d":"2.53"},{"v":2.5280763576980925,"d":"2.53"},{"v":0.912870024,"d":"0.91"}]
["16035","Clearwater","ID",{"v":2.7551717097027018,"d":"2.76"},{"v":2.7551717097027018,"d":"2.76"},{"v":1.9537008589999998,"d":"1.95"}]
["16037","Custer","ID",{"v":2.61135679020791,"d":"2.61"},{"v":2.61135679020791,"d":"2.61"},{"v":1.256217217,"d":"1.26"}]
["16039","Elmore","ID",{"v":2.464822295877308,"d":"2.46"},{"v":2.464822295877308,"d":"2.46"},{"v":0.65600349,"d":"0.66"}]
["16041","Franklin","ID",{"v":2.4795909636612117,"d":"2.48"},{"v":2.479590963661212,"d":"2.48"},{"v":0.799282438,"d":"0.80"}]
["16043","Fremont","ID",{"v":2.514730550110069,"d":"2.51"},{"v":2.514730550110069,"d":"2.51"},{"v":0.87037151,"d":"0.87"}]
["16045","Gem","ID",{"v":2.2277098523392933,"d":"2.23"},{"v":2.2277098523392933,"d":"2.23"},{"v":0.361713362,"d":"0.36"}]
["16047","Gooding","ID",{"v":2.358965906013801,"d":"2.36"},{"v":2.358965906013801,"d":"2.36"},{"v":0.467614897,"d":"0.47"}]
["16049","Idaho","ID",{"v":2.720221228849913,"d":"2.72"},{"v":2.720221228849913,"d":"2.72"},{"v":1.7893971549999999,"d":"1.79"}]
["16051","Jefferson","ID",{"v":2.445024881795889,"d":"2.45"},{"v":2.4450248817958884,"d":"2.45"},{"v":0.587360392,"d":"0.59"}]
["16053","Jerome","ID",{"v":2.3404671354829394,"d":"2.34"},{"v":2.34046713548294,"d":"2.34"},{"v":0.43657769,"d":"0.44"}]
["16055","Kootenai","ID",{"v":2.420767822538077,"d":"2.42"},{"v":2.4207678225380764,"d":"2.42"},{"v":0.823459857,"d":"0.82"}]
["16057","Latah","ID",{"v":2.298668193447034,"d":"2.30"},{"v":2.2986681934470345,"d":"2.30"},{"v":0.557526657,"d":"0.56"}]
["16059","Lemhi","ID",{"v":2.677769937211261,"d":"2.68"},{"v":2.6777699372112616,"d":"2.68"},{"v":1.44895298,"d":"1.45"}]
["16061","Lewis","ID",{"v":2.4048283420292877,"d":"2.40"},{"v":2.4048283420292877,"d":"2.40"},{"v":0.665760247,"d":"0.67"}]
["16063","Lincoln","ID",{"v":2.3951111775055045,"d":"2.40"},{"v":2.3951111775055045,"d":"2.40"},{"v":0.535200125,"d":"0.54"}]
["16065","Madison","ID",{"v":2.4107982368410386,"d":"2.41"},{"v":2.4107982368410386,"d":"2.41"},{"v":0.573578857,"d":"0.57"}]
["16067","Minidoka","ID",{"v":2.3359825096622817,"d":"2.34"},{"v":2.335982509662282,"d":"2.34"},{"v":0.45407049,"d":"0.45"}]
["16069","Nez Perce","ID",{"v":2.334439848257156,"d":"2.33"},{"v":2.3344398482571562,"d":"2.33"},{"v":0.416567529,"d":"0.42"}]
["16071","Oneida","ID",{"v":2.537428009594562,"d":"2.54"},{"v":2.537428009594562,"d":"2.54"},{"v":0.9383804970000001,"d":"0.94"}]
["16073","Owyhee","ID",{"v":2.4355996639420256,"d":"2.44"},{"v":2.435599663942026,"d":"2.44"},{"v":0.61366968,"d":"0.61"}]
["16075","Payette","ID",{"v":2.2229162369341484,"d":"2.22"},{"v":2.222916236934148,"d":"2.22"},{"v":0.30952441,"d":"0.31"}]
["16077","Power","ID",{"v":2.4193891318314997,"d":"2.42"},{"v":2.4193891318314997,"d":"2.42"},{"v":0.558787238,"d":"0.56"}]
["16079","Shoshone","ID",{"v":2.6141272448833726,"d":"2.61"},{"v":2.6141272448833726,"d":"2.61"},{"v":1.462228825,"d":"1.46"}]
["16081","Teton","ID",{"v":2.580378301238012,"d":"2.58"},{"v":2.5803783012380115,"d":"2.58"},{"v":1.213168173,"d":"1.21"}]
["16083","Twin Falls","ID",{"v":2.2905375310999982,"d":"2.29"},{"v":2.2905375310999987,"d":"2.29"},{"v":0.377296494,"d":"0.38"}]
["16085","Valley","ID",{"v":2.620700166495091,"d":"2.62"},{"v":2.6207001664950904,"d":"2.62"},{"v":1.377083743,"d":"1.38"}]
["16087","Washington","ID",{"v":2.225862432662437,"d":"2.23"},{"v":2.225862432662437,"d":"2.23"},{"v":0.340085287,"d":"0.34"}]
["17001","Adams","IL",{"v":2.895240295406728,"d":"2.90"},{"v":2.8952402954067273,"d":"2.90"},{"v":0.378401091,"d":"0.38"}]
["17003","Alexander","IL",{"v":3.162954010077679,"d":"3.16"},{"v":3.162954010077679,"d":"3.16"},{"v":0.45046412799999996,"d":"0.45"}]
["17005","Bond","IL",{"v":3.0050669447538545,"d":"3.01"},{"v":3.005066944753855,"d":"3.01"},{"v":0.410880207,"d":"0.41"}]
["17007","Boone","IL",{"v":2.989587025803807,"d":"2.99"},{"v":2.989587025803807,"d":"2.99"},{"v":0.333899948,"d":"0.33"}]
["17009","Brown","IL",{"v":3.01911690137158,"d":"3.02"},{"v":3.019116901371579,"d":"3.02"},{"v":0.553541623,"d":"0.55"}]
["17011","Bureau","IL",{"v":2.9035024295336247,"d":"2.90"},{"v":2.903502429533625,"d":"2.90"},{"v":0.409757864,"d":"0.41"}]
["17013","Calhoun","IL",{"v":3.2269691969503573,"d":"3.23"},{"v":3.2269691969503578,"d":"3.23"},{"v":0.580349779,"d":"0.58"}]
["17015","Carroll","IL",{"v":3.079557883092828,"d":"3.08"},{"v":3.0795578830928285,"d":"3.08"},{"v":0.512663592,"d":"0.51"}]
["17017","Cass","IL",{"v":2.992839926698346,"d":"2.99"},{"v":2.9928399266983456,"d":"2.99"},{"v":0.345160887,"d":"0.35"}]
["17019","Champaign","IL",{"v":2.565288806172421,"d":"2.57"},{"v":2.565288806172421,"d":"2.57"},{"v":0.29313671,"d":"0.29"}]
["17021","Christian","IL",{"v":2.7590579759315457,"d":"2.76"},{"v":2.759057975931546,"d":"2.76"},{"v":0.264309948,"d":"0.26"}]
["17023","Clark","IL",{"v":2.8936616185330197,"d":"2.89"},{"v":2.89366161853302,"d":"2.89"},{"v":0.380828767,"d":"0.38"}]
["17025","Clay","IL",{"v":3.1518488433008427,"d":"3.15"},{"v":3.1518488433008423,"d":"3.15"},{"v":0.382903078,"d":"0.38"}]
["17027","Clinton","IL",{"v":2.809666585651249,"d":"2.81"},{"v":2.8096665856512493,"d":"2.81"},{"v":0.270657803,"d":"0.27"}]
["17029","Coles","IL",{"v":2.822333377373872,"d":"2.82"},{"v":2.8223333773738726,"d":"2.82"},{"v":0.28240384,"d":"0.28"}]
["17031","Cook","IL",{"v":3.79646082403172e-07,"d":"0.00"},{"v":3.7964608240317203E-7,"d":"0.00"},{"v":6.377594184,"d":"6.38"}]
["17033","Crawford","IL",{"v":2.976772270735163,"d":"2.98"},{"v":2.976772270735163,"d":"2.98"},{"v":0.354051576,"d":"0.35"}]
["17035","Cumberland","IL",{"v":2.991282978990767,"d":"2.99"},{"v":2.991282978990767,"d":"2.99"},{"v":0.444822497,"d":"0.44"}]
["17037","De Kalb","IL",{"v":3.035267094845553,"d":"3.04"},{"v":3.035267094845553,"d":"3.04"},{"v":0.33133853,"d":"0.33"}]
["17039","Dewitt","IL",{"v":2.5100609911641074,"d":"2.51"},{"v":2.5100609911641074,"d":"2.51"},{"v":0.314333827,"d":"0.31"}]
["17041","Douglas","IL",{"v":2.7841903970093047,"d":"2.78"},{"v":2.784190397009305,"d":"2.78"},{"v":0.289970349,"d":"0.29"}]
["17043","Du Page","IL",{"v":0.0126609522873453,"d":"0.01"},{"v":0.012660952287345302,"d":"0.01"},{"v":1.406683182,"d":"1.41"}]
["17045","Edgar","IL",{"v":2.4236492547865827,"d":"2.42"},{"v":2.423649254786583,"d":"2.42"},{"v":0.298725874,"d":"0.30"}]
["17047","Edwards","IL",{"v":2.8047709725413665,"d":"2.80"},{"v":2.8047709725413665,"d":"2.80"},{"v":0.325808691,"d":"0.33"}]
["17049","Effingham","IL",{"v":3.103189749323006,"d":"3.10"},{"v":3.1031897493230054,"d":"3.10"},{"v":0.381127197,"d":"0.38"}]
["17051","Fayette","IL",{"v":3.19662859111846,"d":"3.20"},{"v":3.1966285911184595,"d":"3.20"},{"v":0.401269149,"d":"0.40"}]
["17053","Ford","IL",{"v":3.105359109472209,"d":"3.11"},{"v":3.105359109472209,"d":"3.11"},{"v":0.303605047,"d":"0.30"}]
["17055","Franklin","IL",{"v":2.9463046842251517,"d":"2.95"},{"v":2.9463046842251517,"d":"2.95"},{"v":0.334458195,"d":"0.33"}]
["17057","Fulton","IL",{"v":2.824331770753396,"d":"2.82"},{"v":2.824331770753396,"d":"2.82"},{"v":0.4511625369999999,"d":"0.45"}]
["17059","Gallatin","IL",{"v":2.8140186806572047,"d":"2.81"},{"v":2.814018680657205,"d":"2.81"},{"v":0.355304648,"d":"0.36"}]
["17061","Greene","IL",{"v":2.9794035380481665,"d":"2.98"},{"v":2.9794035380481665,"d":"2.98"},{"v":0.38239749,"d":"0.38"}]
["17063","Grundy","IL",{"v":2.908089362490764,"d":"2.91"},{"v":2.908089362490764,"d":"2.91"},{"v":0.339464388,"d":"0.34"}]
["17065","Hamilton","IL",{"v":3.0013806543814323,"d":"3.00"},{"v":3.0013806543814323,"d":"3.00"},{"v":0.32334881,"d":"0.32"}]
["17067","Hancock","IL",{"v":3.018918411448271,"d":"3.02"},{"v":3.0189184114482708,"d":"3.02"},{"v":0.432882708,"d":"0.43"}]
["17069","Hardin","IL",{"v":3.145196024010862,"d":"3.15"},{"v":3.1451960240108625,"d":"3.15"},{"v":0.629405056,"d":"0.63"}]
["17071","Henderson","IL",{"v":2.91891297129236,"d":"2.92"},{"v":2.91891297129236,"d":"2.92"},{"v":0.425327406,"d":"0.43"}]
["17073","Henry","IL",{"v":2.9158651321301416,"d":"2.92"},{"v":2.915865132130141,"d":"2.92"},{"v":0.390387385,"d":"0.39"}]
["17075","Iroquois","IL",{"v":2.7176766628743247,"d":"2.72"},{"v":2.7176766628743247,"d":"2.72"},{"v":0.358105203,"d":"0.36"}]
["17077","Jackson","IL",{"v":3.0042508160006896,"d":"3.00"},{"v":3.0042508160006887,"d":"3.00"},{"v":0.432705262,"d":"0.43"}]
["17079","Jasper","IL",{"v":3.0423621178395117,"d":"3.04"},{"v":3.0423621178395117,"d":"3.04"},{"v":0.385962219,"d":"0.39"}]
["17081","Jefferson","IL",{"v":2.9974662249822495,"d":"3.00"},{"v":2.9974662249822495,"d":"3.00"},{"v":0.352710018,"d":"0.35"}]
["17083","Jersey","IL",{"v":2.945274481646065,"d":"2.95"},{"v":2.9452744816460656,"d":"2.95"},{"v":0.474470991,"d":"0.47"}]
["17085","Jo Daviess","IL",{"v":2.971478281542796,"d":"2.97"},{"v":2.971478281542796,"d":"2.97"},{"v":0.558291351,"d":"0.56"}]
["17087","Johnson","IL",{"v":3.2370910348600868,"d":"3.24"},{"v":3.2370910348600868,"d":"3.24"},{"v":0.6565525710000001,"d":"0.66"}]
["17089","Kane","IL",{"v":2.3828261210703623,"d":"2.38"},{"v":2.3828261210703627,"d":"2.38"},{"v":0.454443954,"d":"0.45"}]
["17091","Kankakee","IL",{"v":2.764370556944372,"d":"2.76"},{"v":2.764370556944372,"d":"2.76"},{"v":0.289428709,"d":"0.29"}]
["17093","Kendall","IL",{"v":2.9995183225424134,"d":"3.00"},{"v":2.9995183225424134,"d":"3.00"},{"v":0.324637676,"d":"0.32"}]
["17095","Knox","IL",{"v":2.8474104948394077,"d":"2.85"},{"v":2.8474104948394072,"d":"2.85"},{"v":0.327056827,"d":"0.33"}]
["17097","Lake","IL",{"v":1.1160122789076594,"d":"1.12"},{"v":1.1160122789076596,"d":"1.12"},{"v":0.688211855,"d":"0.69"}]
["17099","La Salle","IL",{"v":2.6367595414331455,"d":"2.64"},{"v":2.636759541433146,"d":"2.64"},{"v":0.335042619,"d":"0.34"}]
["17101","Lawrence","IL",{"v":2.770680503912737,"d":"2.77"},{"v":2.7706805039127373,"d":"2.77"},{"v":0.319595407,"d":"0.32"}]
["17103","Lee","IL",{"v":2.8799465417063184,"d":"2.88"},{"v":2.879946541706319,"d":"2.88"},{"v":0.405557688,"d":"0.41"}]
["17105","Livingston","IL",{"v":2.6975823608793976,"d":"2.70"},{"v":2.6975823608793976,"d":"2.70"},{"v":0.303131257,"d":"0.30"}]
["17107","Logan","IL",{"v":2.7341331797675417,"d":"2.73"},{"v":2.734133179767541,"d":"2.73"},{"v":0.304526473,"d":"0.30"}]
["17109","McDonough","IL",{"v":2.8890209652925787,"d":"2.89"},{"v":2.8890209652925787,"d":"2.89"},{"v":0.347985504,"d":"0.35"}]
["17111","McHenry","IL",{"v":2.920063823427,"d":"2.92"},{"v":2.920063823427,"d":"2.92"},{"v":0.381130149,"d":"0.38"}]
["17113","Mclean","IL",{"v":2.6917266733154643,"d":"2.69"},{"v":2.6917266733154643,"d":"2.69"},{"v":0.26375875,"d":"0.26"}]
["17115","Macon","IL",{"v":2.375131529968616,"d":"2.38"},{"v":2.375131529968616,"d":"2.38"},{"v":0.270261692,"d":"0.27"}]
["17117","Macoupin","IL",{"v":2.7500884402463606,"d":"2.75"},{"v":2.75008844024636,"d":"2.75"},{"v":0.3663151820000001,"d":"0.37"}]
["17119","Madison","IL",{"v":2.612930626202279,"d":"2.61"},{"v":2.6129306262022793,"d":"2.61"},{"v":0.314989717,"d":"0.31"}]
["17121","Marion","IL",{"v":3.0428476922271437,"d":"3.04"},{"v":3.0428476922271437,"d":"3.04"},{"v":0.354536001,"d":"0.35"}]
["17123","Marshall","IL",{"v":2.9706845108956537,"d":"2.97"},{"v":2.9706845108956537,"d":"2.97"},{"v":0.415633697,"d":"0.42"}]
["17125","Mason","IL",{"v":3.129798512856494,"d":"3.13"},{"v":3.1297985128564934,"d":"3.13"},{"v":0.402023901,"d":"0.40"}]
["17127","Massac","IL",{"v":2.975646467611429,"d":"2.98"},{"v":2.975646467611429,"d":"2.98"},{"v":0.368461028,"d":"0.37"}]
["17129","Menard","IL",{"v":2.6958913747687174,"d":"2.70"},{"v":2.6958913747687174,"d":"2.70"},{"v":0.386954759,"d":"0.39"}]
["17131","Mercer","IL",{"v":3.037105829557007,"d":"3.04"},{"v":3.037105829557007,"d":"3.04"},{"v":0.492043526,"d":"0.49"}]
["17133","Monroe","IL",{"v":2.906201132627804,"d":"2.91"},{"v":2.9062011326278037,"d":"2.91"},{"v":0.318626121,"d":"0.32"}]
["17135","Montgomery","IL",{"v":2.7807229918889496,"d":"2.78"},{"v":2.7807229918889496,"d":"2.78"},{"v":0.302723462,"d":"0.30"}]
["17137","Morgan","IL",{"v":2.671325977808355,"d":"2.67"},{"v":2.671325977808355,"d":"2.67"},{"v":0.29661846,"d":"0.30"}]
["17139","Moultrie","IL",{"v":2.63640657731846,"d":"2.64"},{"v":2.63640657731846,"d":"2.64"},{"v":0.310132554,"d":"0.31"}]
["17141","Ogle","IL",{"v":3.035291235914227,"d":"3.04"},{"v":3.0352912359142263,"d":"3.04"},{"v":0.4296059850000001,"d":"0.43"}]
["17143","Peoria","IL",{"v":2.808288871538842,"d":"2.81"},{"v":2.8082888715388417,"d":"2.81"},{"v":0.366704655,"d":"0.37"}]
["17145","Perry","IL",{"v":2.9886211990498057,"d":"2.99"},{"v":2.9886211990498053,"d":"2.99"},{"v":0.319060046,"d":"0.32"}]
["17147","Piatt","IL",{"v":2.7845702877880876,"d":"2.78"},{"v":2.784570287788087,"d":"2.78"},{"v":0.337860319,"d":"0.34"}]
["17149","Pike","IL",{"v":2.9147287854749298,"d":"2.91"},{"v":2.9147287854749298,"d":"2.91"},{"v":0.397428307,"d":"0.40"}]
["17151","Pope","IL",{"v":3.1471533980463273,"d":"3.15"},{"v":3.147153398046328,"d":"3.15"},{"v":0.675846458,"d":"0.68"}]
["17153","Pulaski","IL",{"v":3.0390081863855904,"d":"3.04"},{"v":3.03900818638559,"d":"3.04"},{"v":0.42379034700000007,"d":"0.42"}]
["17155","Putnam","IL",{"v":3.1495323297152273,"d":"3.15"},{"v":3.149532329715227,"d":"3.15"},{"v":0.536270728,"d":"0.54"}]
["17157","Randolph","IL",{"v":2.897632636455096,"d":"2.90"},{"v":2.897632636455096,"d":"2.90"},{"v":0.323265525,"d":"0.32"}]
["17159","Richland","IL",{"v":3.032456567308837,"d":"3.03"},{"v":3.0324565673088375,"d":"3.03"},{"v":0.304637142,"d":"0.30"}]
["17161","Rock Island","IL",{"v":2.746267071882957,"d":"2.75"},{"v":2.746267071882957,"d":"2.75"},{"v":0.393294251,"d":"0.39"}]
["17163","St Clair","IL",{"v":2.69353883933404,"d":"2.69"},{"v":2.69353883933404,"d":"2.69"},{"v":0.257091598,"d":"0.26"}]
["17165","Saline","IL",{"v":2.7687868528385384,"d":"2.77"},{"v":2.7687868528385384,"d":"2.77"},{"v":0.328251615,"d":"0.33"}]
["17167","Sangamon","IL",{"v":2.5844305036252524,"d":"2.58"},{"v":2.584430503625252,"d":"2.58"},{"v":0.250214837,"d":"0.25"}]
["17169","Schuyler","IL",{"v":3.210350851685752,"d":"3.21"},{"v":3.210350851685752,"d":"3.21"},{"v":0.516767847,"d":"0.52"}]
["17171","Scott","IL",{"v":2.9695688755549283,"d":"2.97"},{"v":2.969568875554928,"d":"2.97"},{"v":0.413787547,"d":"0.41"}]
["17173","Shelby","IL",{"v":2.903874409057492,"d":"2.90"},{"v":2.9038744090574924,"d":"2.90"},{"v":0.350291232,"d":"0.35"}]
["17175","Stark","IL",{"v":2.94862772516713,"d":"2.95"},{"v":2.94862772516713,"d":"2.95"},{"v":0.401872411,"d":"0.40"}]
["17177","Stephenson","IL",{"v":2.805212349187168,"d":"2.81"},{"v":2.805212349187168,"d":"2.81"},{"v":0.401843669,"d":"0.40"}]
["17179","Tazewell","IL",{"v":2.7612142316964774,"d":"2.76"},{"v":2.761214231696478,"d":"2.76"},{"v":0.304328743,"d":"0.30"}]
["17181","Union","IL",{"v":3.064002715117347,"d":"3.06"},{"v":3.0640027151173466,"d":"3.06"},{"v":0.552580158,"d":"0.55"}]
["17183","Vermilion","IL",{"v":2.8896060377735053,"d":"2.89"},{"v":2.8896060377735058,"d":"2.89"},{"v":0.330819898,"d":"0.33"}]
["17185","Wabash","IL",{"v":2.9388000439221087,"d":"2.94"},{"v":2.938800043922109,"d":"2.94"},{"v":0.259186506,"d":"0.26"}]
["17187","Warren","IL",{"v":3.035801513318923,"d":"3.04"},{"v":3.035801513318923,"d":"3.04"},{"v":0.347840744,"d":"0.35"}]
["17189","Washington","IL",{"v":3.028240220726728,"d":"3.03"},{"v":3.028240220726728,"d":"3.03"},{"v":0.337735221,"d":"0.34"}]
["17191","Wayne","IL",{"v":3.063955113096903,"d":"3.06"},{"v":3.063955113096903,"d":"3.06"},{"v":0.316006514,"d":"0.32"}]
["17193","White","IL",{"v":2.957676185018794,"d":"2.96"},{"v":2.9576761850187943,"d":"2.96"},{"v":0.286444524,"d":"0.29"}]
["17195","Whiteside","IL",{"v":2.9161402385245574,"d":"2.92"},{"v":2.9161402385245574,"d":"2.92"},{"v":0.38113296900000004,"d":"0.38"}]
["17197","Will","IL",{"v":2.597027634116779,"d":"2.60"},{"v":2.5970276341167784,"d":"2.60"},{"v":0.400003779,"d":"0.40"}]
["17199","Williamson","IL",{"v":2.8464324273382866,"d":"2.85"},{"v":2.8464324273382866,"d":"2.85"},{"v":0.422550367,"d":"0.42"}]
["17201","Winnebago","IL",{"v":2.6271058434735406,"d":"2.63"},{"v":2.6271058434735406,"d":"2.63"},{"v":0.40348943400000004,"d":"0.40"}]
["17203","Woodford","IL",{"v":3.009502361738156,"d":"3.01"},{"v":3.009502361738156,"d":"3.01"},{"v":0.352448313,"d":"0.35"}]
["18001","Adams","IN",{"v":3.137437524160933,"d":"3.14"},{"v":3.1374375241609327,"d":"3.14"},{"v":0.416458513,"d":"0.42"}]
["18003","Allen","IN",{"v":2.6501869108257567,"d":"2.65"},{"v":2.650186910825757,"d":"2.65"},{"v":0.391338551,"d":"0.39"}]
["18005","Bartholomew","IN",{"v":3.0318363419845453,"d":"3.03"},{"v":3.0318363419845453,"d":"3.03"},{"v":0.406022873,"d":"0.41"}]
["18007","Benton","IN",{"v":2.8855315738484033,"d":"2.89"},{"v":2.8855315738484033,"d":"2.89"},{"v":0.439314719,"d":"0.44"}]
["18009","Blackford","IN",{"v":3.284453892374986,"d":"3.28"},{"v":3.2844538923749864,"d":"3.28"},{"v":0.39887007900000004,"d":"0.40"}]
["18011","Boone","IN",{"v":2.88159767689637,"d":"2.88"},{"v":2.88159767689637,"d":"2.88"},{"v":0.334538775,"d":"0.33"}]
["18013","Brown","IN",{"v":3.306854108939258,"d":"3.31"},{"v":3.306854108939258,"d":"3.31"},{"v":0.879199992,"d":"0.88"}]
["18015","Carroll","IN",{"v":2.9453311911144326,"d":"2.95"},{"v":2.9453311911144335,"d":"2.95"},{"v":0.497787558,"d":"0.50"}]
["18017","Cass","IN",{"v":2.9476321636611513,"d":"2.95"},{"v":2.9476321636611518,"d":"2.95"},{"v":0.393785693,"d":"0.39"}]
["18019","Clark","IN",{"v":2.8125042138876113,"d":"2.81"},{"v":2.8125042138876113,"d":"2.81"},{"v":0.409404225,"d":"0.41"}]
["18021","Clay","IN",{"v":3.1086618399099453,"d":"3.11"},{"v":3.1086618399099453,"d":"3.11"},{"v":0.54378143,"d":"0.54"}]
["18023","Clinton","IN",{"v":2.9175952612377984,"d":"2.92"},{"v":2.9175952612377984,"d":"2.92"},{"v":0.340736807,"d":"0.34"}]
["18025","Crawford","IN",{"v":3.163937968984271,"d":"3.16"},{"v":3.1639379689842713,"d":"3.16"},{"v":0.778756114,"d":"0.78"}]
["18027","Daviess","IN",{"v":3.009775220522934,"d":"3.01"},{"v":3.0097752205229336,"d":"3.01"},{"v":0.34000173899999997,"d":"0.34"}]
["18029","Dearborn","IN",{"v":3.122757937455451,"d":"3.12"},{"v":3.1227579374554515,"d":"3.12"},{"v":0.539491558,"d":"0.54"}]
["18031","Decatur","IN",{"v":3.13284104481766,"d":"3.13"},{"v":3.132841044817659,"d":"3.13"},{"v":0.43243243900000006,"d":"0.43"}]
["18033","De Kalb","IN",{"v":2.9544672783125665,"d":"2.95"},{"v":2.954467278312566,"d":"2.95"},{"v":0.434395866,"d":"0.43"}]
["18035","Delaware","IN",{"v":2.9652105031382705,"d":"2.97"},{"v":2.965210503138271,"d":"2.97"},{"v":0.341770478,"d":"0.34"}]
["18037","Dubois","IN",{"v":3.104388262213721,"d":"3.10"},{"v":3.1043882622137207,"d":"3.10"},{"v":0.407259485,"d":"0.41"}]
["18039","Elkhart","IN",{"v":2.8573594811700547,"d":"2.86"},{"v":2.8573594811700547,"d":"2.86"},{"v":0.385589367,"d":"0.39"}]
["18041","Fayette","IN",{"v":2.6557231364630347,"d":"2.66"},{"v":2.6557231364630347,"d":"2.66"},{"v":0.402035661,"d":"0.40"}]
["18043","Floyd","IN",{"v":2.9766207669680576,"d":"2.98"},{"v":2.9766207669680576,"d":"2.98"},{"v":0.473751221,"d":"0.47"}]
["18045","Fountain","IN",{"v":3.0049338119026014,"d":"3.00"},{"v":3.004933811902602,"d":"3.00"},{"v":0.437021905,"d":"0.44"}]
["18047","Franklin","IN",{"v":3.127199629446751,"d":"3.13"},{"v":3.1271996294467517,"d":"3.13"},{"v":0.6339205400000001,"d":"0.63"}]
["18049","Fulton","IN",{"v":2.785765771123999,"d":"2.79"},{"v":2.785765771123999,"d":"2.79"},{"v":0.447480397,"d":"0.45"}]
["18051","Gibson","IN",{"v":2.553767527096894,"d":"2.55"},{"v":2.553767527096894,"d":"2.55"},{"v":0.323297397,"d":"0.32"}]
["18053","Grant","IN",{"v":2.9317846383178314,"d":"2.93"},{"v":2.9317846383178314,"d":"2.93"},{"v":0.333703154,"d":"0.33"}]
["18055","Greene","IN",{"v":3.0807416900280553,"d":"3.08"},{"v":3.0807416900280558,"d":"3.08"},{"v":0.451554438,"d":"0.45"}]
["18057","Hamilton","IN",{"v":2.6233874173963896,"d":"2.62"},{"v":2.6233874173963896,"d":"2.62"},{"v":0.38571686099999997,"d":"0.39"}]
["18059","Hancock","IN",{"v":3.0914111390473487,"d":"3.09"},{"v":3.091411139047348,"d":"3.09"},{"v":0.328477299,"d":"0.33"}]
["18061","Harrison","IN",{"v":3.2906942846788843,"d":"3.29"},{"v":3.2906942846788843,"d":"3.29"},{"v":0.631891563,"d":"0.63"}]
["18063","Hendricks","IN",{"v":2.9006020127170116,"d":"2.90"},{"v":2.9006020127170116,"d":"2.90"},{"v":0.3674249479999999,"d":"0.37"}]
["18065","Henry","IN",{"v":2.9173009859470347,"d":"2.92"},{"v":2.9173009859470342,"d":"2.92"},{"v":0.364816388,"d":"0.36"}]
["18067","Howard","IN",{"v":2.820264692850517,"d":"2.82"},{"v":2.820264692850517,"d":"2.82"},{"v":0.292399834,"d":"0.29"}]
["18069","Huntington","IN",{"v":2.9418188319825487,"d":"2.94"},{"v":2.9418188319825487,"d":"2.94"},{"v":0.455882361,"d":"0.46"}]
["18071","Jackson","IN",{"v":3.152032709320152,"d":"3.15"},{"v":3.1520327093201517,"d":"3.15"},{"v":0.450680544,"d":"0.45"}]
["18073","Jasper","IN",{"v":3.251915433904418,"d":"3.25"},{"v":3.2519154339044185,"d":"3.25"},{"v":0.441647121,"d":"0.44"}]
["18075","Jay","IN",{"v":3.3216416630203223,"d":"3.32"},{"v":3.321641663020322,"d":"3.32"},{"v":0.390852736,"d":"0.39"}]
["18077","Jefferson","IN",{"v":3.0331730862642705,"d":"3.03"},{"v":3.0331730862642696,"d":"3.03"},{"v":0.535980448,"d":"0.54"}]
["18079","Jennings","IN",{"v":2.8776826206754307,"d":"2.88"},{"v":2.8776826206754302,"d":"2.88"},{"v":0.574240857,"d":"0.57"}]
["18081","Johnson","IN",{"v":2.6472415573151524,"d":"2.65"},{"v":2.6472415573151524,"d":"2.65"},{"v":0.358047425,"d":"0.36"}]
["18083","Knox","IN",{"v":2.938248173362281,"d":"2.94"},{"v":2.9382481733622816,"d":"2.94"},{"v":0.278679887,"d":"0.28"}]
["18085","Kosciusko","IN",{"v":2.89604593393646,"d":"2.90"},{"v":2.89604593393646,"d":"2.90"},{"v":0.41333586,"d":"0.41"}]
["18087","Lagrange","IN",{"v":2.975909666863665,"d":"2.98"},{"v":2.975909666863665,"d":"2.98"},{"v":0.555085918,"d":"0.56"}]
["18089","Lake","IN",{"v":2.3499588549580994,"d":"2.35"},{"v":2.3499588549580994,"d":"2.35"},{"v":0.43784452,"d":"0.44"}]
["18091","La Porte","IN",{"v":2.8278150065562553,"d":"2.83"},{"v":2.8278150065562553,"d":"2.83"},{"v":0.387135221,"d":"0.39"}]
["18093","Lawrence","IN",{"v":3.1271875012256323,"d":"3.13"},{"v":3.1271875012256323,"d":"3.13"},{"v":0.51123676,"d":"0.51"}]
["18095","Madison","IN",{"v":2.919442969451874,"d":"2.92"},{"v":2.9194429694518744,"d":"2.92"},{"v":0.314571262,"d":"0.31"}]
["18097","Marion","IN",{"v":0.041914818829969676,"d":"0.04"},{"v":0.041914818829969676,"d":"0.04"},{"v":0.977786273,"d":"0.98"}]
["18099","Marshall","IN",{"v":2.8566008991111604,"d":"2.86"},{"v":2.8566008991111604,"d":"2.86"},{"v":0.427386657,"d":"0.43"}]
["18101","Martin","IN",{"v":3.1107302902748293,"d":"3.11"},{"v":3.1107302902748293,"d":"3.11"},{"v":0.622732341,"d":"0.62"}]
["18103","Miami","IN",{"v":2.826390042416377,"d":"2.83"},{"v":2.8263900424163775,"d":"2.83"},{"v":0.421417016,"d":"0.42"}]
["18105","Monroe","IN",{"v":3.039033089779048,"d":"3.04"},{"v":3.039033089779049,"d":"3.04"},{"v":0.514487477,"d":"0.51"}]
["18107","Montgomery","IN",{"v":2.7411603090143344,"d":"2.74"},{"v":2.7411603090143344,"d":"2.74"},{"v":0.394068256,"d":"0.39"}]
["18109","Morgan","IN",{"v":2.7143941443859827,"d":"2.71"},{"v":2.7143941443859827,"d":"2.71"},{"v":0.541192448,"d":"0.54"}]
["18111","Newton","IN",{"v":3.2291455263742863,"d":"3.23"},{"v":3.229145526374286,"d":"3.23"},{"v":0.468172419,"d":"0.47"}]
["18113","Noble","IN",{"v":3.4249415592524777,"d":"3.42"},{"v":3.4249415592524772,"d":"3.42"},{"v":0.538985854,"d":"0.54"}]
["18115","Ohio","IN",{"v":3.0894540680027562,"d":"3.09"},{"v":3.089454068002756,"d":"3.09"},{"v":0.672471724,"d":"0.67"}]
["18117","Orange","IN",{"v":3.269454323222929,"d":"3.27"},{"v":3.269454323222929,"d":"3.27"},{"v":0.582530237,"d":"0.58"}]
["18119","Owen","IN",{"v":3.3640683168546857,"d":"3.36"},{"v":3.3640683168546857,"d":"3.36"},{"v":0.8098976590000001,"d":"0.81"}]
["18121","Parke","IN",{"v":3.2996975550617615,"d":"3.30"},{"v":3.2996975550617615,"d":"3.30"},{"v":0.614400396,"d":"0.61"}]
["18123","Perry","IN",{"v":3.1980438386854084,"d":"3.20"},{"v":3.1980438386854084,"d":"3.20"},{"v":0.561276344,"d":"0.56"}]
["18125","Pike","IN",{"v":3.16723293988582,"d":"3.17"},{"v":3.16723293988582,"d":"3.17"},{"v":0.479842371,"d":"0.48"}]
["18127","Porter","IN",{"v":2.995190133357312,"d":"3.00"},{"v":2.995190133357312,"d":"3.00"},{"v":0.374719106,"d":"0.37"}]
["18129","Posey","IN",{"v":3.2345163277925297,"d":"3.23"},{"v":3.2345163277925297,"d":"3.23"},{"v":0.344006379,"d":"0.34"}]
["18131","Pulaski","IN",{"v":2.9691813987247504,"d":"2.97"},{"v":2.969181398724751,"d":"2.97"},{"v":0.500587521,"d":"0.50"}]
["18133","Putnam","IN",{"v":3.345285340667235,"d":"3.35"},{"v":3.3452853406672345,"d":"3.35"},{"v":0.573939711,"d":"0.57"}]
["18135","Randolph","IN",{"v":2.956028523370412,"d":"2.96"},{"v":2.9560285233704118,"d":"2.96"},{"v":0.405844283,"d":"0.41"}]
["18137","Ripley","IN",{"v":3.197712405736812,"d":"3.20"},{"v":3.197712405736812,"d":"3.20"},{"v":0.539407736,"d":"0.54"}]
["18139","Rush","IN",{"v":2.9751528512711856,"d":"2.98"},{"v":2.975152851271186,"d":"2.98"},{"v":0.383114869,"d":"0.38"}]
["18141","St Joseph","IN",{"v":2.633359500743323,"d":"2.63"},{"v":2.6333595007433224,"d":"2.63"},{"v":0.39103043899999995,"d":"0.39"}]
["18143","Scott","IN",{"v":3.1229686391830658,"d":"3.12"},{"v":3.1229686391830658,"d":"3.12"},{"v":0.509278668,"d":"0.51"}]
["18145","Shelby","IN",{"v":2.969744187659335,"d":"2.97"},{"v":2.9697441876593347,"d":"2.97"},{"v":0.380342021,"d":"0.38"}]
["18147","Spencer","IN",{"v":3.2512768713757407,"d":"3.25"},{"v":3.2512768713757407,"d":"3.25"},{"v":0.432442468,"d":"0.43"}]
["18149","Starke","IN",{"v":2.9632752010628116,"d":"2.96"},{"v":2.963275201062811,"d":"2.96"},{"v":0.478523031,"d":"0.48"}]
["18151","Steuben","IN",{"v":3.313826536154056,"d":"3.31"},{"v":3.3138265361540564,"d":"3.31"},{"v":0.52102349,"d":"0.52"}]
["18153","Sullivan","IN",{"v":3.1157924310978142,"d":"3.12"},{"v":3.1157924310978142,"d":"3.12"},{"v":0.394136152,"d":"0.39"}]
["18155","Switzerland","IN",{"v":3.3440666236063903,"d":"3.34"},{"v":3.3440666236063907,"d":"3.34"},{"v":0.7654453329999998,"d":"0.77"}]
["18157","Tippecanoe","IN",{"v":2.826777696796599,"d":"2.83"},{"v":2.826777696796599,"d":"2.83"},{"v":0.354417766,"d":"0.35"}]
["18159","Tipton","IN",{"v":2.931958509201333,"d":"2.93"},{"v":2.9319585092013325,"d":"2.93"},{"v":0.359631751,"d":"0.36"}]
["18161","Union","IN",{"v":3.0799834632491523,"d":"3.08"},{"v":3.0799834632491523,"d":"3.08"},{"v":0.599309587,"d":"0.60"}]
["18163","Vanderburgh","IN",{"v":2.465630108687723,"d":"2.47"},{"v":2.465630108687723,"d":"2.47"},{"v":0.356521198,"d":"0.36"}]
["18165","Vermillion","IN",{"v":3.277388744524902,"d":"3.28"},{"v":3.277388744524902,"d":"3.28"},{"v":0.476771703,"d":"0.48"}]
["18167","Vigo","IN",{"v":3.098438788645733,"d":"3.10"},{"v":3.0984387886457334,"d":"3.10"},{"v":0.43384553,"d":"0.43"}]
["18169","Wabash","IN",{"v":2.9609524848510813,"d":"2.96"},{"v":2.9609524848510818,"d":"2.96"},{"v":0.432376118,"d":"0.43"}]
["18171","Warren","IN",{"v":3.034015994219205,"d":"3.03"},{"v":3.034015994219205,"d":"3.03"},{"v":0.488637931,"d":"0.49"}]
["18173","Warrick","IN",{"v":2.777542440633286,"d":"2.78"},{"v":2.777542440633286,"d":"2.78"},{"v":0.342753207,"d":"0.34"}]
["18175","Washington","IN",{"v":3.436827501432983,"d":"3.44"},{"v":3.436827501432983,"d":"3.44"},{"v":0.558811209,"d":"0.56"}]
["18177","Wayne","IN",{"v":2.8425273011542904,"d":"2.84"},{"v":2.8425273011542904,"d":"2.84"},{"v":0.39023605,"d":"0.39"}]
["18179","Wells","IN",{"v":3.3013716526929113,"d":"3.30"},{"v":3.301371652692911,"d":"3.30"},{"v":0.416788185,"d":"0.42"}]
["18181","White","IN",{"v":2.966571812799686,"d":"2.97"},{"v":2.9665718127996863,"d":"2.97"},{"v":0.400034413,"d":"0.40"}]
["18183","Whitley","IN",{"v":3.089623073345085,"d":"3.09"},{"v":3.0896230733450847,"d":"3.09"},{"v":0.49466481200000006,"d":"0.49"}]
["19001","Adair","IA",{"v":2.280733675631995,"d":"2.28"},{"v":2.280733675631995,"d":"2.28"},{"v":0.37891232,"d":"0.38"}]
["19003","Adams","IA",{"v":2.2413755869106975,"d":"2.24"},{"v":2.2413755869106975,"d":"2.24"},{"v":0.402690435,"d":"0.40"}]
["19005","Allamakee","IA",{"v":2.4763357680923535,"d":"2.48"},{"v":2.476335768092353,"d":"2.48"},{"v":0.67562707,"d":"0.68"}]
["19007","Appanoose","IA",{"v":2.3509386217444863,"d":"2.35"},{"v":2.350938621744486,"d":"2.35"},{"v":0.403097586,"d":"0.40"}]
["19009","Audubon","IA",{"v":2.1631562755916596,"d":"2.16"},{"v":2.16315627559166,"d":"2.16"},{"v":0.433680714,"d":"0.43"}]
["19011","Benton","IA",{"v":2.323480313409522,"d":"2.32"},{"v":2.3234803134095223,"d":"2.32"},{"v":0.380935874,"d":"0.38"}]
["19013","Black Hawk","IA",{"v":2.2408087615068837,"d":"2.24"},{"v":2.2408087615068832,"d":"2.24"},{"v":0.350066675,"d":"0.35"}]
["19015","Boone","IA",{"v":2.401089893078941,"d":"2.40"},{"v":2.401089893078941,"d":"2.40"},{"v":0.363804127,"d":"0.36"}]
["19017","Bremer","IA",{"v":2.312858695175927,"d":"2.31"},{"v":2.312858695175927,"d":"2.31"},{"v":0.449572857,"d":"0.45"}]
["19019","Buchanan","IA",{"v":2.371214940739969,"d":"2.37"},{"v":2.371214940739969,"d":"2.37"},{"v":0.438835365,"d":"0.44"}]
["19021","Buena Vista","IA",{"v":2.4300219100795712,"d":"2.43"},{"v":2.4300219100795712,"d":"2.43"},{"v":0.423122637,"d":"0.42"}]
["19023","Butler","IA",{"v":2.364418788481578,"d":"2.36"},{"v":2.364418788481578,"d":"2.36"},{"v":0.549652483,"d":"0.55"}]
["19025","Calhoun","IA",{"v":1.7958060653203216,"d":"1.80"},{"v":1.7958060653203212,"d":"1.80"},{"v":0.415400598,"d":"0.42"}]
["19027","Carroll","IA",{"v":1.8412053593885356,"d":"1.84"},{"v":1.8412053593885358,"d":"1.84"},{"v":0.363282802,"d":"0.36"}]
["19029","Cass","IA",{"v":2.1517091839710907,"d":"2.15"},{"v":2.1517091839710907,"d":"2.15"},{"v":0.296174917,"d":"0.30"}]
["19031","Cedar","IA",{"v":2.3344803037976685,"d":"2.33"},{"v":2.3344803037976685,"d":"2.33"},{"v":0.393387031,"d":"0.39"}]
["19033","Cerro Gordo","IA",{"v":2.382586982773425,"d":"2.38"},{"v":2.3825869827734256,"d":"2.38"},{"v":0.344397847,"d":"0.34"}]
["19035","Cherokee","IA",{"v":2.4622546386866695,"d":"2.46"},{"v":2.462254638686669,"d":"2.46"},{"v":0.46718343900000003,"d":"0.47"}]
["19037","Chickasaw","IA",{"v":2.446395366256213,"d":"2.45"},{"v":2.446395366256213,"d":"2.45"},{"v":0.479131411,"d":"0.48"}]
["19039","Clarke","IA",{"v":2.2787179450544195,"d":"2.28"},{"v":2.2787179450544195,"d":"2.28"},{"v":0.392542528,"d":"0.39"}]
["19041","Clay","IA",{"v":2.3231141709763268,"d":"2.32"},{"v":2.3231141709763268,"d":"2.32"},{"v":0.405925499,"d":"0.41"}]
["19043","Clayton","IA",{"v":2.4724414179290513,"d":"2.47"},{"v":2.4724414179290517,"d":"2.47"},{"v":0.649115791,"d":"0.65"}]
["19045","Clinton","IA",{"v":2.155481079407769,"d":"2.16"},{"v":2.155481079407769,"d":"2.16"},{"v":0.306396717,"d":"0.31"}]
["19047","Crawford","IA",{"v":2.373243880797198,"d":"2.37"},{"v":2.3732438807971974,"d":"2.37"},{"v":0.426835309,"d":"0.43"}]
["19049","Dallas","IA",{"v":2.372096370327773,"d":"2.37"},{"v":2.372096370327773,"d":"2.37"},{"v":0.346593634,"d":"0.35"}]
["19051","Davis","IA",{"v":2.3869025176614977,"d":"2.39"},{"v":2.3869025176614977,"d":"2.39"},{"v":0.491784456,"d":"0.49"}]
["19053","Decatur","IA",{"v":2.2837412158483645,"d":"2.28"},{"v":2.2837412158483645,"d":"2.28"},{"v":0.465110965,"d":"0.47"}]
["19055","Delaware","IA",{"v":2.4315770265461967,"d":"2.43"},{"v":2.4315770265461967,"d":"2.43"},{"v":0.470558259,"d":"0.47"}]
["19057","Des Moines","IA",{"v":2.2369411817000393,"d":"2.24"},{"v":2.2369411817000397,"d":"2.24"},{"v":0.29403751,"d":"0.29"}]
["19059","Dickinson","IA",{"v":2.439541122361629,"d":"2.44"},{"v":2.4395411223616286,"d":"2.44"},{"v":0.396308541,"d":"0.40"}]
["19061","Dubuque","IA",{"v":2.3834601836235545,"d":"2.38"},{"v":2.3834601836235545,"d":"2.38"},{"v":0.40325677,"d":"0.40"}]
["19063","Emmet","IA",{"v":2.3171039331537227,"d":"2.32"},{"v":2.317103933153723,"d":"2.32"},{"v":0.391078721,"d":"0.39"}]
["19065","Fayette","IA",{"v":2.4008650335046307,"d":"2.40"},{"v":2.400865033504631,"d":"2.40"},{"v":0.472949952,"d":"0.47"}]
["19067","Floyd","IA",{"v":2.451206642215773,"d":"2.45"},{"v":2.451206642215773,"d":"2.45"},{"v":0.440339589,"d":"0.44"}]
["19069","Franklin","IA",{"v":2.3657067271804286,"d":"2.37"},{"v":2.3657067271804286,"d":"2.37"},{"v":0.47962941000000003,"d":"0.48"}]
["19071","Fremont","IA",{"v":2.272118637699281,"d":"2.27"},{"v":2.2721186376992804,"d":"2.27"},{"v":0.400746203,"d":"0.40"}]
["19073","Greene","IA",{"v":2.2449746440806466,"d":"2.24"},{"v":2.2449746440806466,"d":"2.24"},{"v":0.373926146,"d":"0.37"}]
["19075","Grundy","IA",{"v":1.9922212408277675,"d":"1.99"},{"v":1.9922212408277677,"d":"1.99"},{"v":0.404504898,"d":"0.40"}]
["19077","Guthrie","IA",{"v":2.4260033973407813,"d":"2.43"},{"v":2.426003397340781,"d":"2.43"},{"v":0.46664717699999997,"d":"0.47"}]
["19079","Hamilton","IA",{"v":2.365222688899061,"d":"2.37"},{"v":2.3652226888990606,"d":"2.37"},{"v":0.337762249,"d":"0.34"}]
["19081","Hancock","IA",{"v":2.3221290889625266,"d":"2.32"},{"v":2.3221290889625266,"d":"2.32"},{"v":0.460638706,"d":"0.46"}]
["19083","Hardin","IA",{"v":2.332554099454617,"d":"2.33"},{"v":2.332554099454617,"d":"2.33"},{"v":0.376634158,"d":"0.38"}]
["19085","Harrison","IA",{"v":2.3429356286686844,"d":"2.34"},{"v":2.3429356286686844,"d":"2.34"},{"v":0.482461349,"d":"0.48"}]
["19087","Henry","IA",{"v":2.3401601150280738,"d":"2.34"},{"v":2.3401601150280738,"d":"2.34"},{"v":0.357611305,"d":"0.36"}]
["19089","Howard","IA",{"v":2.4761066779086667,"d":"2.48"},{"v":2.4761066779086667,"d":"2.48"},{"v":0.490333949,"d":"0.49"}]
["19091","Humboldt","IA",{"v":2.429012286777606,"d":"2.43"},{"v":2.429012286777606,"d":"2.43"},{"v":0.44541295099999995,"d":"0.45"}]
["19093","Ida","IA",{"v":1.759054787898159,"d":"1.76"},{"v":1.7590547878981588,"d":"1.76"},{"v":0.440933914,"d":"0.44"}]
["19095","Iowa","IA",{"v":2.218213380838165,"d":"2.22"},{"v":2.218213380838165,"d":"2.22"},{"v":0.399726484,"d":"0.40"}]
["19097","Jackson","IA",{"v":2.2990717564314966,"d":"2.30"},{"v":2.299071756431496,"d":"2.30"},{"v":0.415165829,"d":"0.42"}]
["19099","Jasper","IA",{"v":2.327452893476501,"d":"2.33"},{"v":2.3274528934765013,"d":"2.33"},{"v":0.372626161,"d":"0.37"}]
["19101","Jefferson","IA",{"v":2.311058305828111,"d":"2.31"},{"v":2.3110583058281113,"d":"2.31"},{"v":0.329852376,"d":"0.33"}]
["19103","Johnson","IA",{"v":2.3045038882664906,"d":"2.30"},{"v":2.304503888266491,"d":"2.30"},{"v":0.307890007,"d":"0.31"}]
["19105","Jones","IA",{"v":2.3084491494208725,"d":"2.31"},{"v":2.3084491494208725,"d":"2.31"},{"v":0.41048775,"d":"0.41"}]
["19107","Keokuk","IA",{"v":2.273425803715527,"d":"2.27"},{"v":2.2734258037155266,"d":"2.27"},{"v":0.428806034,"d":"0.43"}]
["19109","Kossuth","IA",{"v":2.3138980768610042,"d":"2.31"},{"v":2.3138980768610042,"d":"2.31"},{"v":0.45690991700000005,"d":"0.46"}]
["19111","Lee","IA",{"v":2.367454872041297,"d":"2.37"},{"v":2.367454872041297,"d":"2.37"},{"v":0.365684537,"d":"0.37"}]
["19113","Linn","IA",{"v":2.2376809729979534,"d":"2.24"},{"v":2.2376809729979534,"d":"2.24"},{"v":0.290336089,"d":"0.29"}]
["19115","Louisa","IA",{"v":2.129847362059694,"d":"2.13"},{"v":2.129847362059694,"d":"2.13"},{"v":0.40165859600000003,"d":"0.40"}]
["19117","Lucas","IA",{"v":2.307914434482975,"d":"2.31"},{"v":2.307914434482975,"d":"2.31"},{"v":0.39347605,"d":"0.39"}]
["19119","Lyon","IA",{"v":2.454149376294855,"d":"2.45"},{"v":2.454149376294855,"d":"2.45"},{"v":0.533578928,"d":"0.53"}]
["19121","Madison","IA",{"v":2.3054081358136798,"d":"2.31"},{"v":2.30540813581368,"d":"2.31"},{"v":0.390924549,"d":"0.39"}]
["19123","Mahaska","IA",{"v":2.2074201704440943,"d":"2.21"},{"v":2.2074201704440943,"d":"2.21"},{"v":0.300649878,"d":"0.30"}]
["19125","Marion","IA",{"v":2.3047679429312673,"d":"2.30"},{"v":2.3047679429312677,"d":"2.30"},{"v":0.32575062,"d":"0.33"}]
["19127","Marshall","IA",{"v":2.264103512865496,"d":"2.26"},{"v":2.2641035128654954,"d":"2.26"},{"v":0.333022888,"d":"0.33"}]
["19129","Mills","IA",{"v":2.2438972377261606,"d":"2.24"},{"v":2.2438972377261606,"d":"2.24"},{"v":0.360355914,"d":"0.36"}]
["19131","Mitchell","IA",{"v":2.4509055653934446,"d":"2.45"},{"v":2.4509055653934446,"d":"2.45"},{"v":0.501379283,"d":"0.50"}]
["19133","Monona","IA",{"v":2.349048697784594,"d":"2.35"},{"v":2.349048697784594,"d":"2.35"},{"v":0.472853663,"d":"0.47"}]
["19135","Monroe","IA",{"v":2.366203314361882,"d":"2.37"},{"v":2.366203314361882,"d":"2.37"},{"v":0.41836982,"d":"0.42"}]
["19137","Montgomery","IA",{"v":2.177074755313549,"d":"2.18"},{"v":2.177074755313549,"d":"2.18"},{"v":0.302555201,"d":"0.30"}]
["19139","Muscatine","IA",{"v":2.2179183985246396,"d":"2.22"},{"v":2.2179183985246396,"d":"2.22"},{"v":0.29681588,"d":"0.30"}]
["19141","Obrien","IA",{"v":2.003467141903405,"d":"2.00"},{"v":2.003467141903405,"d":"2.00"},{"v":0.446036174,"d":"0.45"}]
["19143","Osceola","IA",{"v":2.0880209866470163,"d":"2.09"},{"v":2.0880209866470163,"d":"2.09"},{"v":0.46940778,"d":"0.47"}]
["19145","Page","IA",{"v":2.2037735787785038,"d":"2.20"},{"v":2.2037735787785038,"d":"2.20"},{"v":0.297397587,"d":"0.30"}]
["19147","Palo Alto","IA",{"v":2.2656986248448794,"d":"2.27"},{"v":2.265698624844879,"d":"2.27"},{"v":0.448450913,"d":"0.45"}]
["19149","Plymouth","IA",{"v":2.389476155343081,"d":"2.39"},{"v":2.389476155343081,"d":"2.39"},{"v":0.471613152,"d":"0.47"}]
["19151","Pocahontas","IA",{"v":2.0359217070905697,"d":"2.04"},{"v":2.0359217070905693,"d":"2.04"},{"v":0.515231376,"d":"0.52"}]
["19153","Polk","IA",{"v":1.8407705760200124,"d":"1.84"},{"v":1.8407705760200124,"d":"1.84"},{"v":0.397271955,"d":"0.40"}]
["19155","Pottawattamie","IA",{"v":2.2378622228562763,"d":"2.24"},{"v":2.237862222856276,"d":"2.24"},{"v":0.257134725,"d":"0.26"}]
["19157","Poweshiek","IA",{"v":2.3780332321521462,"d":"2.38"},{"v":2.3780332321521462,"d":"2.38"},{"v":0.384768417,"d":"0.38"}]
["19159","Ringgold","IA",{"v":2.2814328739871885,"d":"2.28"},{"v":2.2814328739871885,"d":"2.28"},{"v":0.441885223,"d":"0.44"}]
["19161","Sac","IA",{"v":2.2759196645319846,"d":"2.28"},{"v":2.2759196645319846,"d":"2.28"},{"v":0.436227843,"d":"0.44"}]
["19163","Scott","IA",{"v":2.1595643046467385,"d":"2.16"},{"v":2.159564304646738,"d":"2.16"},{"v":0.305209329,"d":"0.31"}]
["19165","Shelby","IA",{"v":2.267824730948265,"d":"2.27"},{"v":2.267824730948265,"d":"2.27"},{"v":0.39459971799999993,"d":"0.39"}]
["19167","Sioux","IA",{"v":1.913076764151102,"d":"1.91"},{"v":1.9130767641511022,"d":"1.91"},{"v":0.4545519,"d":"0.45"}]
["19169","Story","IA",{"v":2.31682406618573,"d":"2.32"},{"v":2.31682406618573,"d":"2.32"},{"v":0.298955473,"d":"0.30"}]
["19171","Tama","IA",{"v":2.3114598344902486,"d":"2.31"},{"v":2.3114598344902486,"d":"2.31"},{"v":0.417645239,"d":"0.42"}]
["19173","Taylor","IA",{"v":2.3018227874594226,"d":"2.30"},{"v":2.301822787459422,"d":"2.30"},{"v":0.434037163,"d":"0.43"}]
["19175","Union","IA",{"v":2.220029963585751,"d":"2.22"},{"v":2.220029963585751,"d":"2.22"},{"v":0.309655344,"d":"0.31"}]
["19177","Van Buren","IA",{"v":2.437094996031696,"d":"2.44"},{"v":2.437094996031696,"d":"2.44"},{"v":0.526957142,"d":"0.53"}]
["19179","Wapello","IA",{"v":2.276542992270739,"d":"2.28"},{"v":2.276542992270739,"d":"2.28"},{"v":0.306588621,"d":"0.31"}]
["19181","Warren","IA",{"v":2.2933350330816924,"d":"2.29"},{"v":2.2933350330816924,"d":"2.29"},{"v":0.346647322,"d":"0.35"}]
["19183","Washington","IA",{"v":2.230643494906525,"d":"2.23"},{"v":2.230643494906525,"d":"2.23"},{"v":0.360011052,"d":"0.36"}]
["19185","Wayne","IA",{"v":2.3356794676972794,"d":"2.34"},{"v":2.3356794676972794,"d":"2.34"},{"v":0.438097129,"d":"0.44"}]
["19187","Webster","IA",{"v":2.3567176700595627,"d":"2.36"},{"v":2.3567176700595622,"d":"2.36"},{"v":0.309121679,"d":"0.31"}]
["19189","Winnebago","IA",{"v":2.416234772663266,"d":"2.42"},{"v":2.416234772663266,"d":"2.42"},{"v":0.46824909700000006,"d":"0.47"}]
["19191","Winneshiek","IA",{"v":2.4394218663389955,"d":"2.44"},{"v":2.4394218663389955,"d":"2.44"},{"v":0.517908883,"d":"0.52"}]
["19193","Woodbury","IA",{"v":2.3309656941929746,"d":"2.33"},{"v":2.330965694192974,"d":"2.33"},{"v":0.308397262,"d":"0.31"}]
["19195","Worth","IA",{"v":2.432457685598,"d":"2.43"},{"v":2.432457685598,"d":"2.43"},{"v":0.529581963,"d":"0.53"}]
["19197","Wright","IA",{"v":2.423749984160741,"d":"2.42"},{"v":2.423749984160741,"d":"2.42"},{"v":0.437420259,"d":"0.44"}]
["20001","Allen","KS",{"v":2.6268376889801432,"d":"2.63"},{"v":2.6268376889801432,"d":"2.63"},{"v":0.272492649,"d":"0.27"}]
["20003","Anderson","KS",{"v":2.785892356336206,"d":"2.79"},{"v":2.785892356336206,"d":"2.79"},{"v":0.333513254,"d":"0.33"}]
["20005","Atchison","KS",{"v":2.7971860261598427,"d":"2.80"},{"v":2.7971860261598427,"d":"2.80"},{"v":0.33360313,"d":"0.33"}]
["20007","Barber","KS",{"v":2.4436016551785196,"d":"2.44"},{"v":2.443601655178519,"d":"2.44"},{"v":0.292338857,"d":"0.29"}]
["20009","Barton","KS",{"v":2.4406700355030226,"d":"2.44"},{"v":2.4406700355030226,"d":"2.44"},{"v":0.234076138,"d":"0.23"}]
["20011","Bourbon","KS",{"v":2.6351522510385115,"d":"2.64"},{"v":2.635152251038511,"d":"2.64"},{"v":0.288323282,"d":"0.29"}]
["20013","Brown","KS",{"v":2.7234162102473203,"d":"2.72"},{"v":2.72341621024732,"d":"2.72"},{"v":0.344417467,"d":"0.34"}]
["20015","Butler","KS",{"v":2.5753773731402227,"d":"2.58"},{"v":2.5753773731402227,"d":"2.58"},{"v":0.24338906900000004,"d":"0.24"}]
["20017","Chase","KS",{"v":2.949440381671335,"d":"2.95"},{"v":2.9494403816713346,"d":"2.95"},{"v":0.335105557,"d":"0.34"}]
["20019","Chautauqua","KS",{"v":3.0646592304370768,"d":"3.06"},{"v":3.0646592304370768,"d":"3.06"},{"v":0.337535207,"d":"0.34"}]
["20021","Cherokee","KS",{"v":2.68932071292287,"d":"2.69"},{"v":2.68932071292287,"d":"2.69"},{"v":0.306532675,"d":"0.31"}]
["20023","Cheyenne","KS",{"v":2.896863055744282,"d":"2.90"},{"v":2.8968630557442823,"d":"2.90"},{"v":0.348122038,"d":"0.35"}]
["20025","Clark","KS",{"v":2.7537616882345253,"d":"2.75"},{"v":2.7537616882345253,"d":"2.75"},{"v":0.270447415,"d":"0.27"}]
["20027","Clay","KS",{"v":2.772677019745902,"d":"2.77"},{"v":2.772677019745902,"d":"2.77"},{"v":0.323322923,"d":"0.32"}]
["20029","Cloud","KS",{"v":2.975385258464176,"d":"2.98"},{"v":2.9753852584641765,"d":"2.98"},{"v":0.299319274,"d":"0.30"}]
["20031","Coffey","KS",{"v":2.901334664980955,"d":"2.90"},{"v":2.9013346649809546,"d":"2.90"},{"v":0.334839577,"d":"0.33"}]
["20033","Comanche","KS",{"v":2.8090070937656675,"d":"2.81"},{"v":2.809007093765667,"d":"2.81"},{"v":0.297182824,"d":"0.30"}]
["20035","Cowley","KS",{"v":2.5787714567840223,"d":"2.58"},{"v":2.5787714567840228,"d":"2.58"},{"v":0.227417796,"d":"0.23"}]
["20037","Crawford","KS",{"v":2.549001092842971,"d":"2.55"},{"v":2.549001092842971,"d":"2.55"},{"v":0.251207338,"d":"0.25"}]
["20039","Decatur","KS",{"v":2.8998311085793365,"d":"2.90"},{"v":2.899831108579337,"d":"2.90"},{"v":0.359702042,"d":"0.36"}]
["20041","Dickinson","KS",{"v":2.690486044309377,"d":"2.69"},{"v":2.690486044309377,"d":"2.69"},{"v":0.297368841,"d":"0.30"}]
["20043","Doniphan","KS",{"v":2.555136818665624,"d":"2.56"},{"v":2.5551368186656243,"d":"2.56"},{"v":0.406319739,"d":"0.41"}]
["20045","Douglas","KS",{"v":2.546743085451949,"d":"2.55"},{"v":2.546743085451949,"d":"2.55"},{"v":0.279802807,"d":"0.28"}]
["20047","Edwards","KS",{"v":2.754745960564508,"d":"2.75"},{"v":2.754745960564508,"d":"2.75"},{"v":0.27201621,"d":"0.27"}]
["20049","Elk","KS",{"v":3.023347504551772,"d":"3.02"},{"v":3.0233475045517726,"d":"3.02"},{"v":0.299865554,"d":"0.30"}]
["20051","Ellis","KS",{"v":2.690539467207268,"d":"2.69"},{"v":2.6905394672072678,"d":"2.69"},{"v":0.23189130399999996,"d":"0.23"}]
["20053","Ellsworth","KS",{"v":2.8291063619350862,"d":"2.83"},{"v":2.8291063619350862,"d":"2.83"},{"v":0.284908969,"d":"0.28"}]
["20055","Finney","KS",{"v":2.369687564505996,"d":"2.37"},{"v":2.369687564505996,"d":"2.37"},{"v":0.184783839,"d":"0.18"}]
["20057","Ford","KS",{"v":2.3116643685985476,"d":"2.31"},{"v":2.311664368598548,"d":"2.31"},{"v":0.202316867,"d":"0.20"}]
["20059","Franklin","KS",{"v":2.774031897475604,"d":"2.77"},{"v":2.774031897475604,"d":"2.77"},{"v":0.328207152,"d":"0.33"}]
["20061","Geary","KS",{"v":2.6785265392054347,"d":"2.68"},{"v":2.6785265392054343,"d":"2.68"},{"v":0.265333275,"d":"0.27"}]
["20063","Gove","KS",{"v":2.8792995659810394,"d":"2.88"},{"v":2.87929956598104,"d":"2.88"},{"v":0.334689302,"d":"0.33"}]
["20065","Graham","KS",{"v":2.858143170922738,"d":"2.86"},{"v":2.8581431709227374,"d":"2.86"},{"v":0.343548004,"d":"0.34"}]
["20067","Grant","KS",{"v":2.7756993301740103,"d":"2.78"},{"v":2.7756993301740103,"d":"2.78"},{"v":0.195412897,"d":"0.20"}]
["20069","Gray","KS",{"v":2.1124441851322557,"d":"2.11"},{"v":2.1124441851322553,"d":"2.11"},{"v":0.260585459,"d":"0.26"}]
["20071","Greeley","KS",{"v":2.8799161379283875,"d":"2.88"},{"v":2.8799161379283875,"d":"2.88"},{"v":0.320331707,"d":"0.32"}]
["20073","Greenwood","KS",{"v":2.7363558941891992,"d":"2.74"},{"v":2.736355894189199,"d":"2.74"},{"v":0.276318372,"d":"0.28"}]
["20075","Hamilton","KS",{"v":2.6541821829471757,"d":"2.65"},{"v":2.6541821829471752,"d":"2.65"},{"v":0.252625073,"d":"0.25"}]
["20077","Harper","KS",{"v":2.52870608470983,"d":"2.53"},{"v":2.5287060847098295,"d":"2.53"},{"v":0.274772552,"d":"0.27"}]
["20079","Harvey","KS",{"v":2.4086616015563096,"d":"2.41"},{"v":2.40866160155631,"d":"2.41"},{"v":0.22604925200000003,"d":"0.23"}]
["20081","Haskell","KS",{"v":2.7980564238038874,"d":"2.80"},{"v":2.7980564238038874,"d":"2.80"},{"v":0.26363991,"d":"0.26"}]
["20083","Hodgeman","KS",{"v":2.806840258102763,"d":"2.81"},{"v":2.806840258102763,"d":"2.81"},{"v":0.310234357,"d":"0.31"}]
["20085","Jackson","KS",{"v":3.0839459924256265,"d":"3.08"},{"v":3.083945992425626,"d":"3.08"},{"v":0.457019735,"d":"0.46"}]
["20087","Jefferson","KS",{"v":3.0021643427519313,"d":"3.00"},{"v":3.0021643427519313,"d":"3.00"},{"v":0.522357492,"d":"0.52"}]
["20089","Jewell","KS",{"v":2.96456922206398,"d":"2.96"},{"v":2.96456922206398,"d":"2.96"},{"v":0.388423875,"d":"0.39"}]
["20091","Johnson","KS",{"v":1.518546218232188,"d":"1.52"},{"v":1.5185462182321883,"d":"1.52"},{"v":0.41637226299999996,"d":"0.42"}]
["20093","Kearny","KS",{"v":2.7222029605846885,"d":"2.72"},{"v":2.7222029605846885,"d":"2.72"},{"v":0.253687339,"d":"0.25"}]
["20095","Kingman","KS",{"v":2.6288886923367616,"d":"2.63"},{"v":2.628888692336761,"d":"2.63"},{"v":0.276731861,"d":"0.28"}]
["20097","Kiowa","KS",{"v":1.9839718883705373,"d":"1.98"},{"v":1.9839718883705368,"d":"1.98"},{"v":0.289381769,"d":"0.29"}]
["20099","Labette","KS",{"v":2.588149969482486,"d":"2.59"},{"v":2.588149969482486,"d":"2.59"},{"v":0.26516587,"d":"0.27"}]
["20101","Lane","KS",{"v":2.87030431685678,"d":"2.87"},{"v":2.87030431685678,"d":"2.87"},{"v":0.318234599,"d":"0.32"}]
["20103","Leavenworth","KS",{"v":3.0151552788872436,"d":"3.02"},{"v":3.0151552788872436,"d":"3.02"},{"v":0.382593138,"d":"0.38"}]
["20105","Lincoln","KS",{"v":2.869551818946192,"d":"2.87"},{"v":2.8695518189461917,"d":"2.87"},{"v":0.33505959,"d":"0.34"}]
["20107","Linn","KS",{"v":2.841716753774184,"d":"2.84"},{"v":2.8417167537741843,"d":"2.84"},{"v":0.49049120000000007,"d":"0.49"}]
["20109","Logan","KS",{"v":2.796440419769451,"d":"2.80"},{"v":2.796440419769451,"d":"2.80"},{"v":0.302249464,"d":"0.30"}]
["20111","Lyon","KS",{"v":2.6489920630213635,"d":"2.65"},{"v":2.6489920630213635,"d":"2.65"},{"v":0.259841326,"d":"0.26"}]
["20113","McPherson","KS",{"v":2.584093088193129,"d":"2.58"},{"v":2.584093088193129,"d":"2.58"},{"v":0.268521305,"d":"0.27"}]
["20115","Marion","KS",{"v":2.6148104035147517,"d":"2.61"},{"v":2.6148104035147517,"d":"2.61"},{"v":0.31124704,"d":"0.31"}]
["20117","Marshall","KS",{"v":2.7413027447930354,"d":"2.74"},{"v":2.7413027447930354,"d":"2.74"},{"v":0.354768697,"d":"0.35"}]
["20119","Meade","KS",{"v":2.6148269095535572,"d":"2.61"},{"v":2.614826909553557,"d":"2.61"},{"v":0.263234087,"d":"0.26"}]
["20121","Miami","KS",{"v":3.0543769461317916,"d":"3.05"},{"v":3.054376946131792,"d":"3.05"},{"v":0.378639066,"d":"0.38"}]
["20123","Mitchell","KS",{"v":2.551923549945284,"d":"2.55"},{"v":2.5519235499452844,"d":"2.55"},{"v":0.295321165,"d":"0.30"}]
["20125","Montgomery","KS",{"v":2.5556745387503277,"d":"2.56"},{"v":2.5556745387503277,"d":"2.56"},{"v":0.260567328,"d":"0.26"}]
["20127","Morris","KS",{"v":2.8915859726093633,"d":"2.89"},{"v":2.8915859726093633,"d":"2.89"},{"v":0.34980679,"d":"0.35"}]
["20129","Morton","KS",{"v":2.7902274872871207,"d":"2.79"},{"v":2.7902274872871202,"d":"2.79"},{"v":0.277230289,"d":"0.28"}]
["20131","Nemaha","KS",{"v":2.695839057970118,"d":"2.70"},{"v":2.6958390579701175,"d":"2.70"},{"v":0.36611462300000003,"d":"0.37"}]
["20133","Neosho","KS",{"v":2.7671301212257906,"d":"2.77"},{"v":2.7671301212257906,"d":"2.77"},{"v":0.256943942,"d":"0.26"}]
["20135","Ness","KS",{"v":2.2207316491700384,"d":"2.22"},{"v":2.2207316491700384,"d":"2.22"},{"v":0.336102371,"d":"0.34"}]
["20137","Norton","KS",{"v":2.9094437575347554,"d":"2.91"},{"v":2.9094437575347554,"d":"2.91"},{"v":0.30207253,"d":"0.30"}]
["20139","Osage","KS",{"v":2.6914155971183478,"d":"2.69"},{"v":2.691415597118348,"d":"2.69"},{"v":0.369332223,"d":"0.37"}]
["20141","Osborne","KS",{"v":2.5516837180145915,"d":"2.55"},{"v":2.5516837180145915,"d":"2.55"},{"v":0.359997936,"d":"0.36"}]
["20143","Ottawa","KS",{"v":2.6818428773556904,"d":"2.68"},{"v":2.6818428773556904,"d":"2.68"},{"v":0.431888738,"d":"0.43"}]
["20145","Pawnee","KS",{"v":2.52896423388182,"d":"2.53"},{"v":2.52896423388182,"d":"2.53"},{"v":0.209449123,"d":"0.21"}]
["20147","Phillips","KS",{"v":2.900198931445706,"d":"2.90"},{"v":2.9001989314457064,"d":"2.90"},{"v":0.310748527,"d":"0.31"}]
["20149","Pottawatomie","KS",{"v":2.7786720489836196,"d":"2.78"},{"v":2.7786720489836196,"d":"2.78"},{"v":0.369742837,"d":"0.37"}]
["20151","Pratt","KS",{"v":2.509713684934375,"d":"2.51"},{"v":2.509713684934375,"d":"2.51"},{"v":0.214160465,"d":"0.21"}]
["20153","Rawlins","KS",{"v":2.9409188961746384,"d":"2.94"},{"v":2.9409188961746384,"d":"2.94"},{"v":0.373198341,"d":"0.37"}]
["20155","Reno","KS",{"v":2.392961927693104,"d":"2.39"},{"v":2.3929619276931042,"d":"2.39"},{"v":0.224601875,"d":"0.22"}]
["20157","Republic","KS",{"v":3.143897983946108,"d":"3.14"},{"v":3.143897983946108,"d":"3.14"},{"v":0.38031366,"d":"0.38"}]
["20159","Rice","KS",{"v":2.1393087111601052,"d":"2.14"},{"v":2.1393087111601052,"d":"2.14"},{"v":0.28089162,"d":"0.28"}]
["20161","Riley","KS",{"v":2.9708672426999674,"d":"2.97"},{"v":2.970867242699968,"d":"2.97"},{"v":0.323875354,"d":"0.32"}]
["20163","Rooks","KS",{"v":2.871670662369337,"d":"2.87"},{"v":2.8716706623693367,"d":"2.87"},{"v":0.340235546,"d":"0.34"}]
["20165","Rush","KS",{"v":2.821947066427369,"d":"2.82"},{"v":2.8219470664273687,"d":"2.82"},{"v":0.302577852,"d":"0.30"}]
["20167","Russell","KS",{"v":2.6192866541612334,"d":"2.62"},{"v":2.619286654161233,"d":"2.62"},{"v":0.245707563,"d":"0.25"}]
["20169","Saline","KS",{"v":2.510439970103538,"d":"2.51"},{"v":2.510439970103538,"d":"2.51"},{"v":0.22432996200000002,"d":"0.22"}]
["20171","Scott","KS",{"v":2.8265924513951766,"d":"2.83"},{"v":2.8265924513951766,"d":"2.83"},{"v":0.217230161,"d":"0.22"}]
["20173","Sedgwick","KS",{"v":2.3047789398455296,"d":"2.30"},{"v":2.30477893984553,"d":"2.30"},{"v":0.241516693,"d":"0.24"}]
["20175","Seward","KS",{"v":2.6957056025070667,"d":"2.70"},{"v":2.6957056025070667,"d":"2.70"},{"v":0.173743801,"d":"0.17"}]
["20177","Shawnee","KS",{"v":2.6984792037026124,"d":"2.70"},{"v":2.6984792037026124,"d":"2.70"},{"v":0.276393178,"d":"0.28"}]
["20179","Sheridan","KS",{"v":2.84572579513328,"d":"2.85"},{"v":2.84572579513328,"d":"2.85"},{"v":0.353745513,"d":"0.35"}]
["20181","Sherman","KS",{"v":2.591621852534964,"d":"2.59"},{"v":2.591621852534964,"d":"2.59"},{"v":0.24696219400000002,"d":"0.25"}]
["20183","Smith","KS",{"v":2.3918252067277854,"d":"2.39"},{"v":2.3918252067277854,"d":"2.39"},{"v":0.3688178389999999,"d":"0.37"}]
["20185","Stafford","KS",{"v":2.7433160601410065,"d":"2.74"},{"v":2.743316060141006,"d":"2.74"},{"v":0.287418803,"d":"0.29"}]
["20187","Stanton","KS",{"v":2.7925996691611705,"d":"2.79"},{"v":2.7925996691611705,"d":"2.79"},{"v":0.258982807,"d":"0.26"}]
["20189","Stevens","KS",{"v":2.77847104211593,"d":"2.78"},{"v":2.77847104211593,"d":"2.78"},{"v":0.203935528,"d":"0.20"}]
["20191","Sumner","KS",{"v":2.5530089129528863,"d":"2.55"},{"v":2.553008912952886,"d":"2.55"},{"v":0.263478023,"d":"0.26"}]
["20193","Thomas","KS",{"v":2.5584174070196912,"d":"2.56"},{"v":2.5584174070196912,"d":"2.56"},{"v":0.25376065,"d":"0.25"}]
["20195","Trego","KS",{"v":2.0280045498035912,"d":"2.03"},{"v":2.0280045498035912,"d":"2.03"},{"v":0.324431452,"d":"0.32"}]
["20197","Wabaunsee","KS",{"v":3.065758665024658,"d":"3.07"},{"v":3.0657586650246578,"d":"3.07"},{"v":0.372523013,"d":"0.37"}]
["20199","Wallace","KS",{"v":2.5922336096129897,"d":"2.59"},{"v":2.5922336096129897,"d":"2.59"},{"v":0.325923307,"d":"0.33"}]
["20201","Washington","KS",{"v":3.0363257965508925,"d":"3.04"},{"v":3.036325796550892,"d":"3.04"},{"v":0.385077373,"d":"0.39"}]
["20203","Wichita","KS",{"v":2.837930679230729,"d":"2.84"},{"v":2.837930679230729,"d":"2.84"},{"v":0.300044343,"d":"0.30"}]
["20205","Wilson","KS",{"v":2.550989215262301,"d":"2.55"},{"v":2.550989215262301,"d":"2.55"},{"v":0.298706544,"d":"0.30"}]
["20207","Woodson","KS",{"v":2.6916617078570355,"d":"2.69"},{"v":2.6916617078570355,"d":"2.69"},{"v":0.329244547,"d":"0.33"}]
["20209","Wyandotte","KS",{"v":2.2402220065549594,"d":"2.24"},{"v":2.2402220065549594,"d":"2.24"},{"v":0.49738898299999995,"d":"0.50"}]
["21001","Adair","KY",{"v":3.684745751614261,"d":"3.68"},{"v":3.684745751614261,"d":"3.68"},{"v":0.774625201,"d":"0.77"}]
["21003","Allen","KY",{"v":4.242505632586114,"d":"4.24"},{"v":4.242505632586114,"d":"4.24"},{"v":0.69653111,"d":"0.70"}]
["21005","Anderson","KY",{"v":3.948761903899389,"d":"3.95"},{"v":3.9487619038993893,"d":"3.95"},{"v":0.675712609,"d":"0.68"}]
["21007","Ballard","KY",{"v":3.7057682141025827,"d":"3.71"},{"v":3.705768214102583,"d":"3.71"},{"v":0.508531103,"d":"0.51"}]
["21009","Barren","KY",{"v":3.464267703408694,"d":"3.46"},{"v":3.464267703408694,"d":"3.46"},{"v":0.49431088599999995,"d":"0.49"}]
["21011","Bath","KY",{"v":4.409505215789092,"d":"4.41"},{"v":4.409505215789092,"d":"4.41"},{"v":0.813172059,"d":"0.81"}]
["21013","Bell","KY",{"v":4.009203341921512,"d":"4.01"},{"v":4.009203341921512,"d":"4.01"},{"v":1.158657333,"d":"1.16"}]
["21015","Boone","KY",{"v":3.290069823659893,"d":"3.29"},{"v":3.2900698236598926,"d":"3.29"},{"v":0.566716325,"d":"0.57"}]
["21017","Bourbon","KY",{"v":3.378789236294544,"d":"3.38"},{"v":3.378789236294544,"d":"3.38"},{"v":0.400834995,"d":"0.40"}]
["21019","Boyd","KY",{"v":3.8387606376905947,"d":"3.84"},{"v":3.8387606376905947,"d":"3.84"},{"v":0.673927429,"d":"0.67"}]
["21021","Boyle","KY",{"v":3.8953299232954635,"d":"3.90"},{"v":3.8953299232954635,"d":"3.90"},{"v":0.501776,"d":"0.50"}]
["21023","Bracken","KY",{"v":3.5701076141966075,"d":"3.57"},{"v":3.5701076141966075,"d":"3.57"},{"v":0.83891514,"d":"0.84"}]
["21025","Breathitt","KY",{"v":4.2429462628949,"d":"4.24"},{"v":4.2429462628949,"d":"4.24"},{"v":1.273833966,"d":"1.27"}]
["21027","Breckinridge","KY",{"v":3.749655774118242,"d":"3.75"},{"v":3.7496557741182426,"d":"3.75"},{"v":0.744105799,"d":"0.74"}]
["21029","Bullitt","KY",{"v":3.430156807801058,"d":"3.43"},{"v":3.430156807801058,"d":"3.43"},{"v":0.606278631,"d":"0.61"}]
["21031","Butler","KY",{"v":3.7138679715441105,"d":"3.71"},{"v":3.7138679715441105,"d":"3.71"},{"v":0.781126852,"d":"0.78"}]
["21033","Caldwell","KY",{"v":4.090225277359944,"d":"4.09"},{"v":4.090225277359944,"d":"4.09"},{"v":0.557933402,"d":"0.56"}]
["21035","Calloway","KY",{"v":3.998399357386742,"d":"4.00"},{"v":3.998399357386742,"d":"4.00"},{"v":0.514982576,"d":"0.51"}]
["21037","Campbell","KY",{"v":3.2763347933908404,"d":"3.28"},{"v":3.2763347933908404,"d":"3.28"},{"v":0.621161752,"d":"0.62"}]
["21039","Carlisle","KY",{"v":4.009432598744581,"d":"4.01"},{"v":4.0094325987445805,"d":"4.01"},{"v":0.503640287,"d":"0.50"}]
["21041","Carroll","KY",{"v":4.144648181209779,"d":"4.14"},{"v":4.144648181209778,"d":"4.14"},{"v":0.656266395,"d":"0.66"}]
["21043","Carter","KY",{"v":4.183862544031948,"d":"4.18"},{"v":4.183862544031948,"d":"4.18"},{"v":1.148495854,"d":"1.15"}]
["21045","Casey","KY",{"v":4.307206142674765,"d":"4.31"},{"v":4.307206142674765,"d":"4.31"},{"v":0.912912698,"d":"0.91"}]
["21047","Christian","KY",{"v":3.795804510910868,"d":"3.80"},{"v":3.7958045109108682,"d":"3.80"},{"v":0.447611518,"d":"0.45"}]
["21049","Clark","KY",{"v":3.358315395395824,"d":"3.36"},{"v":3.3583153953958242,"d":"3.36"},{"v":0.44874401100000005,"d":"0.45"}]
["21051","Clay","KY",{"v":4.31853728853817,"d":"4.32"},{"v":4.318537288538171,"d":"4.32"},{"v":1.181739558,"d":"1.18"}]
["21053","Clinton","KY",{"v":4.445875926404076,"d":"4.45"},{"v":4.445875926404076,"d":"4.45"},{"v":0.9378721089999998,"d":"0.94"}]
["21055","Crittenden","KY",{"v":3.676658491224425,"d":"3.68"},{"v":3.6766584912244253,"d":"3.68"},{"v":0.613763887,"d":"0.61"}]
["21057","Cumberland","KY",{"v":4.2468478491980814,"d":"4.25"},{"v":4.2468478491980814,"d":"4.25"},{"v":1.057205502,"d":"1.06"}]
["21059","Daviess","KY",{"v":3.6626483307298945,"d":"3.66"},{"v":3.6626483307298945,"d":"3.66"},{"v":0.323164247,"d":"0.32"}]
["21061","Edmonson","KY",{"v":4.495559101854397,"d":"4.50"},{"v":4.495559101854397,"d":"4.50"},{"v":0.949545186,"d":"0.95"}]
["21063","Elliott","KY",{"v":4.381312000073821,"d":"4.38"},{"v":4.381312000073821,"d":"4.38"},{"v":1.30030959,"d":"1.30"}]
["21065","Estill","KY",{"v":4.192186299545319,"d":"4.19"},{"v":4.192186299545318,"d":"4.19"},{"v":0.937143056,"d":"0.94"}]
["21067","Fayette","KY",{"v":2.0531619451792724,"d":"2.05"},{"v":2.0531619451792724,"d":"2.05"},{"v":0.519681301,"d":"0.52"}]
["21069","Fleming","KY",{"v":4.258544999729753,"d":"4.26"},{"v":4.258544999729754,"d":"4.26"},{"v":0.7720069320000001,"d":"0.77"}]
["21071","Floyd","KY",{"v":3.811141066631913,"d":"3.81"},{"v":3.8111410666319125,"d":"3.81"},{"v":1.074214677,"d":"1.07"}]
["21073","Franklin","KY",{"v":3.498489563254399,"d":"3.50"},{"v":3.4984895632543993,"d":"3.50"},{"v":0.530632123,"d":"0.53"}]
["21075","Fulton","KY",{"v":3.08053706068853,"d":"3.08"},{"v":3.08053706068853,"d":"3.08"},{"v":0.40723834100000006,"d":"0.41"}]
["21077","Gallatin","KY",{"v":4.8561965665427165,"d":"4.86"},{"v":4.8561965665427165,"d":"4.86"},{"v":0.915285865,"d":"0.92"}]
["21079","Garrard","KY",{"v":3.5902043362363236,"d":"3.59"},{"v":3.590204336236323,"d":"3.59"},{"v":0.698754254,"d":"0.70"}]
["21081","Grant","KY",{"v":3.593154744284539,"d":"3.59"},{"v":3.593154744284538,"d":"3.59"},{"v":0.835861467,"d":"0.84"}]
["21083","Graves","KY",{"v":3.9709900692362825,"d":"3.97"},{"v":3.9709900692362825,"d":"3.97"},{"v":0.456945603,"d":"0.46"}]
["21085","Grayson","KY",{"v":3.9568259391857574,"d":"3.96"},{"v":3.9568259391857574,"d":"3.96"},{"v":0.7261420729999999,"d":"0.73"}]
["21087","Green","KY",{"v":4.1694222741349085,"d":"4.17"},{"v":4.1694222741349085,"d":"4.17"},{"v":0.669508259,"d":"0.67"}]
["21089","Greenup","KY",{"v":3.621751557273361,"d":"3.62"},{"v":3.6217515572733605,"d":"3.62"},{"v":0.71737423,"d":"0.72"}]
["21091","Hancock","KY",{"v":3.7022846759525225,"d":"3.70"},{"v":3.702284675952522,"d":"3.70"},{"v":0.646062489,"d":"0.65"}]
["21093","Hardin","KY",{"v":3.9095029141832724,"d":"3.91"},{"v":3.9095029141832724,"d":"3.91"},{"v":0.5672669,"d":"0.57"}]
["21095","Harlan","KY",{"v":3.726023906721669,"d":"3.73"},{"v":3.726023906721668,"d":"3.73"},{"v":1.223674434,"d":"1.22"}]
["21097","Harrison","KY",{"v":3.450678627510392,"d":"3.45"},{"v":3.450678627510392,"d":"3.45"},{"v":0.599182706,"d":"0.60"}]
["21099","Hart","KY",{"v":3.9892208314102136,"d":"3.99"},{"v":3.9892208314102136,"d":"3.99"},{"v":0.721436804,"d":"0.72"}]
["21101","Henderson","KY",{"v":3.2282236182563278,"d":"3.23"},{"v":3.2282236182563273,"d":"3.23"},{"v":0.363775939,"d":"0.36"}]
["21103","Henry","KY",{"v":3.445542692398478,"d":"3.45"},{"v":3.4455426923984778,"d":"3.45"},{"v":0.705545802,"d":"0.71"}]
["21105","Hickman","KY",{"v":3.6600356575650115,"d":"3.66"},{"v":3.660035657565012,"d":"3.66"},{"v":0.512474285,"d":"0.51"}]
["21107","Hopkins","KY",{"v":3.506048726944634,"d":"3.51"},{"v":3.506048726944634,"d":"3.51"},{"v":0.513514649,"d":"0.51"}]
["21109","Jackson","KY",{"v":4.459272002701586,"d":"4.46"},{"v":4.459272002701585,"d":"4.46"},{"v":1.237476033,"d":"1.24"}]
["21111","Jefferson","KY",{"v":0.1461795018045355,"d":"0.15"},{"v":0.1461795018045355,"d":"0.15"},{"v":0.8440817489999999,"d":"0.84"}]
["21113","Jessamine","KY",{"v":3.338936603414296,"d":"3.34"},{"v":3.3389366034142958,"d":"3.34"},{"v":0.506207966,"d":"0.51"}]
["21115","Johnson","KY",{"v":4.010947282736144,"d":"4.01"},{"v":4.010947282736144,"d":"4.01"},{"v":1.148809517,"d":"1.15"}]
["21117","Kenton","KY",{"v":2.6152313295152902,"d":"2.62"},{"v":2.6152313295152907,"d":"2.62"},{"v":0.6952761,"d":"0.70"}]
["21119","Knott","KY",{"v":2.9848414369710845,"d":"2.98"},{"v":2.984841436971084,"d":"2.98"},{"v":1.072707272,"d":"1.07"}]
["21121","Knox","KY",{"v":3.9082584923929153,"d":"3.91"},{"v":3.908258492392915,"d":"3.91"},{"v":1.015054949,"d":"1.02"}]
["21123","Larue","KY",{"v":3.481781591901138,"d":"3.48"},{"v":3.4817815919011372,"d":"3.48"},{"v":0.639287785,"d":"0.64"}]
["21125","Laurel","KY",{"v":4.065022820115351,"d":"4.07"},{"v":4.06502282011535,"d":"4.07"},{"v":0.9140207460000002,"d":"0.91"}]
["21127","Lawrence","KY",{"v":3.6107864927491558,"d":"3.61"},{"v":3.6107864927491558,"d":"3.61"},{"v":1.123769761,"d":"1.12"}]
["21129","Lee","KY",{"v":3.9513588050964854,"d":"3.95"},{"v":3.951358805096485,"d":"3.95"},{"v":1.286174791,"d":"1.29"}]
["21131","Leslie","KY",{"v":4.476698069421971,"d":"4.48"},{"v":4.476698069421971,"d":"4.48"},{"v":1.468338405,"d":"1.47"}]
["21133","Letcher","KY",{"v":3.587373706144119,"d":"3.59"},{"v":3.587373706144119,"d":"3.59"},{"v":1.334997518,"d":"1.33"}]
["21135","Lewis","KY",{"v":4.18614934349429,"d":"4.19"},{"v":4.186149343494289,"d":"4.19"},{"v":1.108328045,"d":"1.11"}]
["21137","Lincoln","KY",{"v":4.497444706581737,"d":"4.50"},{"v":4.497444706581737,"d":"4.50"},{"v":0.754074397,"d":"0.75"}]
["21139","Livingston","KY",{"v":4.304387907693448,"d":"4.30"},{"v":4.304387907693448,"d":"4.30"},{"v":0.716174339,"d":"0.72"}]
["21141","Logan","KY",{"v":3.8275383249166652,"d":"3.83"},{"v":3.8275383249166652,"d":"3.83"},{"v":0.503838521,"d":"0.50"}]
["21143","Lyon","KY",{"v":4.215795439946042,"d":"4.22"},{"v":4.215795439946042,"d":"4.22"},{"v":0.75101754,"d":"0.75"}]
["21145","McCracken","KY",{"v":3.890041411797872,"d":"3.89"},{"v":3.8900414117978723,"d":"3.89"},{"v":0.399219687,"d":"0.40"}]
["21147","McCreary","KY",{"v":3.7210609055082964,"d":"3.72"},{"v":3.7210609055082964,"d":"3.72"},{"v":1.396624741,"d":"1.40"}]
["21149","Mclean","KY",{"v":3.4668739543518696,"d":"3.47"},{"v":3.4668739543518696,"d":"3.47"},{"v":0.526205986,"d":"0.53"}]
["21151","Madison","KY",{"v":3.4264180269122013,"d":"3.43"},{"v":3.426418026912201,"d":"3.43"},{"v":0.6488288240000001,"d":"0.65"}]
["21153","Magoffin","KY",{"v":3.8643166034714636,"d":"3.86"},{"v":3.8643166034714636,"d":"3.86"},{"v":1.266030916,"d":"1.27"}]
["21155","Marion","KY",{"v":3.8542281575965354,"d":"3.85"},{"v":3.854228157596535,"d":"3.85"},{"v":0.618763545,"d":"0.62"}]
["21157","Marshall","KY",{"v":4.0331345329918165,"d":"4.03"},{"v":4.0331345329918165,"d":"4.03"},{"v":0.579630069,"d":"0.58"}]
["21159","Martin","KY",{"v":4.443913815435106,"d":"4.44"},{"v":4.443913815435106,"d":"4.44"},{"v":1.047927981,"d":"1.05"}]
["21161","Mason","KY",{"v":3.9284766238373696,"d":"3.93"},{"v":3.9284766238373696,"d":"3.93"},{"v":0.546691384,"d":"0.55"}]
["21163","Meade","KY",{"v":4.220275693362757,"d":"4.22"},{"v":4.220275693362757,"d":"4.22"},{"v":0.746436661,"d":"0.75"}]
["21165","Menifee","KY",{"v":4.347522986107342,"d":"4.35"},{"v":4.347522986107343,"d":"4.35"},{"v":1.176744146,"d":"1.18"}]
["21167","Mercer","KY",{"v":3.415342412390143,"d":"3.42"},{"v":3.4153424123901432,"d":"3.42"},{"v":0.523702065,"d":"0.52"}]
["21169","Metcalfe","KY",{"v":4.084328712651696,"d":"4.08"},{"v":4.084328712651696,"d":"4.08"},{"v":0.682831979,"d":"0.68"}]
["21171","Monroe","KY",{"v":4.072166970824676,"d":"4.07"},{"v":4.072166970824676,"d":"4.07"},{"v":0.705254716,"d":"0.71"}]
["21173","Montgomery","KY",{"v":3.4129950387893637,"d":"3.41"},{"v":3.4129950387893637,"d":"3.41"},{"v":0.587629254,"d":"0.59"}]
["21175","Morgan","KY",{"v":4.149950318358898,"d":"4.15"},{"v":4.149950318358898,"d":"4.15"},{"v":1.263334165,"d":"1.26"}]
["21177","Muhlenberg","KY",{"v":3.590759650789287,"d":"3.59"},{"v":3.5907596507892876,"d":"3.59"},{"v":0.631017916,"d":"0.63"}]
["21179","Nelson","KY",{"v":4.096326261397524,"d":"4.10"},{"v":4.096326261397524,"d":"4.10"},{"v":0.643235368,"d":"0.64"}]
["21181","Nicholas","KY",{"v":3.8697883737710974,"d":"3.87"},{"v":3.8697883737710974,"d":"3.87"},{"v":0.727979127,"d":"0.73"}]
["21183","Ohio","KY",{"v":3.920242108359624,"d":"3.92"},{"v":3.920242108359624,"d":"3.92"},{"v":0.679224794,"d":"0.68"}]
["21185","Oldham","KY",{"v":3.3374009126214426,"d":"3.34"},{"v":3.337400912621442,"d":"3.34"},{"v":0.49957354500000006,"d":"0.50"}]
["21187","Owen","KY",{"v":4.673145153098291,"d":"4.67"},{"v":4.673145153098291,"d":"4.67"},{"v":0.9397395630000002,"d":"0.94"}]
["21189","Owsley","KY",{"v":4.3626762764657885,"d":"4.36"},{"v":4.3626762764657885,"d":"4.36"},{"v":1.370370016,"d":"1.37"}]
["21191","Pendleton","KY",{"v":3.0553713767134414,"d":"3.06"},{"v":3.055371376713442,"d":"3.06"},{"v":0.843959781,"d":"0.84"}]
["21193","Perry","KY",{"v":4.120714550552126,"d":"4.12"},{"v":4.120714550552125,"d":"4.12"},{"v":1.164758642,"d":"1.16"}]
["21195","Pike","KY",{"v":3.9229799773127927,"d":"3.92"},{"v":3.9229799773127922,"d":"3.92"},{"v":1.195833536,"d":"1.20"}]
["21197","Powell","KY",{"v":3.226497971828525,"d":"3.23"},{"v":3.2264979718285245,"d":"3.23"},{"v":0.9958542360000001,"d":"1.00"}]
["21199","Pulaski","KY",{"v":4.197817664375847,"d":"4.20"},{"v":4.197817664375847,"d":"4.20"},{"v":0.789569446,"d":"0.79"}]
["21201","Robertson","KY",{"v":3.905466975488055,"d":"3.91"},{"v":3.905466975488055,"d":"3.91"},{"v":0.9243482630000001,"d":"0.92"}]
["21203","Rockcastle","KY",{"v":4.409353131539408,"d":"4.41"},{"v":4.409353131539408,"d":"4.41"},{"v":1.115403138,"d":"1.12"}]
["21205","Rowan","KY",{"v":4.354246927978634,"d":"4.35"},{"v":4.354246927978634,"d":"4.35"},{"v":1.02352097,"d":"1.02"}]
["21207","Russell","KY",{"v":3.903540198705181,"d":"3.90"},{"v":3.903540198705181,"d":"3.90"},{"v":0.851743919,"d":"0.85"}]
["21209","Scott","KY",{"v":3.6242600284981954,"d":"3.62"},{"v":3.624260028498196,"d":"3.62"},{"v":0.542077516,"d":"0.54"}]
["21211","Shelby","KY",{"v":3.8027016745037976,"d":"3.80"},{"v":3.802701674503797,"d":"3.80"},{"v":0.492448801,"d":"0.49"}]
["21213","Simpson","KY",{"v":3.6834534676286728,"d":"3.68"},{"v":3.6834534676286728,"d":"3.68"},{"v":0.343977316,"d":"0.34"}]
["21215","Spencer","KY",{"v":4.120655180349245,"d":"4.12"},{"v":4.120655180349246,"d":"4.12"},{"v":0.815007198,"d":"0.82"}]
["21217","Taylor","KY",{"v":3.8690206569135,"d":"3.87"},{"v":3.8690206569135,"d":"3.87"},{"v":0.563031552,"d":"0.56"}]
["21219","Todd","KY",{"v":4.251086124505506,"d":"4.25"},{"v":4.251086124505506,"d":"4.25"},{"v":0.570590355,"d":"0.57"}]
["21221","Trigg","KY",{"v":4.0931960367062175,"d":"4.09"},{"v":4.093196036706218,"d":"4.09"},{"v":0.713022512,"d":"0.71"}]
["21223","Trimble","KY",{"v":3.686554506490791,"d":"3.69"},{"v":3.686554506490791,"d":"3.69"},{"v":0.882583623,"d":"0.88"}]
["21225","Union","KY",{"v":3.3941130366879912,"d":"3.39"},{"v":3.394113036687991,"d":"3.39"},{"v":0.441559643,"d":"0.44"}]
["21227","Warren","KY",{"v":3.7474758455179957,"d":"3.75"},{"v":3.7474758455179957,"d":"3.75"},{"v":0.450984342,"d":"0.45"}]
["21229","Washington","KY",{"v":3.5042052996837656,"d":"3.50"},{"v":3.5042052996837656,"d":"3.50"},{"v":0.729008356,"d":"0.73"}]
["21231","Wayne","KY",{"v":4.538197696247647,"d":"4.54"},{"v":4.538197696247647,"d":"4.54"},{"v":1.025061324,"d":"1.03"}]
["21233","Webster","KY",{"v":3.4543426577289122,"d":"3.45"},{"v":3.4543426577289122,"d":"3.45"},{"v":0.545868922,"d":"0.55"}]
["21235","Whitley","KY",{"v":4.080986833668304,"d":"4.08"},{"v":4.080986833668304,"d":"4.08"},{"v":0.933505746,"d":"0.93"}]
["21237","Wolfe","KY",{"v":4.421013022266175,"d":"4.42"},{"v":4.421013022266175,"d":"4.42"},{"v":1.169372885,"d":"1.17"}]
["21239","Woodford","KY",{"v":3.6346318371985604,"d":"3.63"},{"v":3.634631837198561,"d":"3.63"},{"v":0.424820876,"d":"0.42"}]
["22001","Acadia","LA",{"v":0.8372988908242871,"d":"0.84"},{"v":0.8372988908242871,"d":"0.84"},{"v":0.054173835000000004,"d":"0.05"}]
["22003","Allen","LA",{"v":0.8311288897575998,"d":"0.83"},{"v":0.8311288897575998,"d":"0.83"},{"v":0.109046491,"d":"0.11"}]
["22005","Ascension","LA",{"v":0.6972653419373546,"d":"0.70"},{"v":0.6972653419373547,"d":"0.70"},{"v":0.061623186,"d":"0.06"}]
["22007","Assumption","LA",{"v":0.7404613703324183,"d":"0.74"},{"v":0.7404613703324182,"d":"0.74"},{"v":0.074558584,"d":"0.07"}]
["22009","Avoyelles","LA",{"v":0.8699543295332284,"d":"0.87"},{"v":0.8699543295332285,"d":"0.87"},{"v":0.071799554,"d":"0.07"}]
["22011","Beauregard","LA",{"v":0.8185326537135736,"d":"0.82"},{"v":0.8185326537135736,"d":"0.82"},{"v":0.11247999799999998,"d":"0.11"}]
["22013","Bienville","LA",{"v":0.8892870039858687,"d":"0.89"},{"v":0.8892870039858688,"d":"0.89"},{"v":0.144121348,"d":"0.14"}]
["22015","Bossier","LA",{"v":0.8995085300931656,"d":"0.90"},{"v":0.8995085300931654,"d":"0.90"},{"v":0.092021864,"d":"0.09"}]
["22017","Caddo","LA",{"v":0.8252742670383946,"d":"0.83"},{"v":0.8252742670383945,"d":"0.83"},{"v":0.078428879,"d":"0.08"}]
["22019","Calcasieu","LA",{"v":0.8266670524744701,"d":"0.83"},{"v":0.8266670524744701,"d":"0.83"},{"v":0.056872213,"d":"0.06"}]
["22021","Caldwell","LA",{"v":0.9622498599798452,"d":"0.96"},{"v":0.9622498599798452,"d":"0.96"},{"v":0.149613027,"d":"0.15"}]
["22023","Cameron","LA",{"v":0.8669037890903124,"d":"0.87"},{"v":0.8669037890903123,"d":"0.87"},{"v":0.053347690999999996,"d":"0.05"}]
["22025","Catahoula","LA",{"v":0.7842673122191804,"d":"0.78"},{"v":0.7842673122191804,"d":"0.78"},{"v":0.084743444,"d":"0.08"}]
["22027","Claiborne","LA",{"v":0.8408633445459549,"d":"0.84"},{"v":0.8408633445459549,"d":"0.84"},{"v":0.1386392,"d":"0.14"}]
["22029","Concordia","LA",{"v":0.7605247198353343,"d":"0.76"},{"v":0.7605247198353343,"d":"0.76"},{"v":0.05874483,"d":"0.06"}]
["22031","De Soto","LA",{"v":0.9188508759862855,"d":"0.92"},{"v":0.9188508759862853,"d":"0.92"},{"v":0.12496807399999998,"d":"0.12"}]
["22033","East Baton Rouge","LA",{"v":0.6059811871533443,"d":"0.61"},{"v":0.6059811871533444,"d":"0.61"},{"v":0.093823711,"d":"0.09"}]
["22035","East Carroll","LA",{"v":0.6794121291178741,"d":"0.68"},{"v":0.679412129117874,"d":"0.68"},{"v":0.052232577,"d":"0.05"}]
["22037","East Feliciana","LA",{"v":0.847478628557913,"d":"0.85"},{"v":0.847478628557913,"d":"0.85"},{"v":0.12443075199999999,"d":"0.12"}]
["22039","Evangeline","LA",{"v":0.8327290938068436,"d":"0.83"},{"v":0.8327290938068437,"d":"0.83"},{"v":0.081636763,"d":"0.08"}]
["22041","Franklin","LA",{"v":0.8615161071260213,"d":"0.86"},{"v":0.8615161071260212,"d":"0.86"},{"v":0.079701082,"d":"0.08"}]
["22043","Grant","LA",{"v":0.8542797514157057,"d":"0.85"},{"v":0.8542797514157057,"d":"0.85"},{"v":0.138580141,"d":"0.14"}]
["22045","Iberia","LA",{"v":0.8003444953188067,"d":"0.80"},{"v":0.8003444953188067,"d":"0.80"},{"v":0.043970478,"d":"0.04"}]
["22047","Iberville","LA",{"v":0.7433318666540488,"d":"0.74"},{"v":0.7433318666540488,"d":"0.74"},{"v":0.083155882,"d":"0.08"}]
["22049","Jackson","LA",{"v":0.9164919773719357,"d":"0.92"},{"v":0.9164919773719356,"d":"0.92"},{"v":0.138557305,"d":"0.14"}]
["22051","Jefferson","LA",{"v":0.2512494857104702,"d":"0.25"},{"v":0.2512494857104702,"d":"0.25"},{"v":0.056689963,"d":"0.06"}]
["22053","Jefferson Davis","LA",{"v":0.7210238827100386,"d":"0.72"},{"v":0.7210238827100387,"d":"0.72"},{"v":0.050294080000000005,"d":"0.05"}]
["22055","Lafayette","LA",{"v":0.6409351606173653,"d":"0.64"},{"v":0.6409351606173654,"d":"0.64"},{"v":0.06299521,"d":"0.06"}]
["22057","Lafourche","LA",{"v":0.788335418290839,"d":"0.79"},{"v":0.788335418290839,"d":"0.79"},{"v":0.037599949,"d":"0.04"}]
["22059","LaSalle","LA",{"v":0.8936666698852712,"d":"0.89"},{"v":0.893666669885271,"d":"0.89"},{"v":0.128481176,"d":"0.13"}]
["22061","Lincoln","LA",{"v":0.749195842665551,"d":"0.75"},{"v":0.7491958426655508,"d":"0.75"},{"v":0.11364230100000001,"d":"0.11"}]
["22063","Livingston","LA",{"v":0.803213335215464,"d":"0.80"},{"v":0.8032133352154641,"d":"0.80"},{"v":0.10570227,"d":"0.11"}]
["22065","Madison","LA",{"v":0.7969740021701122,"d":"0.80"},{"v":0.7969740021701122,"d":"0.80"},{"v":0.057555218,"d":"0.06"}]
["22067","Morehouse","LA",{"v":0.8630875991223946,"d":"0.86"},{"v":0.8630875991223946,"d":"0.86"},{"v":0.082767426,"d":"0.08"}]
["22069","Natchitoches","LA",{"v":0.9183898083336606,"d":"0.92"},{"v":0.9183898083336607,"d":"0.92"},{"v":0.10573418,"d":"0.11"}]
["22071","Orleans","LA",{"v":0.01090322706202521,"d":"0.01"},{"v":0.01090322706202521,"d":"0.01"},{"v":0.094048401,"d":"0.09"}]
["22073","Ouachita","LA",{"v":0.927183819643342,"d":"0.93"},{"v":0.927183819643342,"d":"0.93"},{"v":0.098871978,"d":"0.10"}]
["22075","Plaquemines","LA",{"v":0.8018706869101078,"d":"0.80"},{"v":0.8018706869101079,"d":"0.80"},{"v":0.030524412,"d":"0.03"}]
["22077","Pointe Coupee","LA",{"v":0.8454407019949446,"d":"0.85"},{"v":0.8454407019949446,"d":"0.85"},{"v":0.068116215,"d":"0.07"}]
["22079","Rapides","LA",{"v":0.8867640806305532,"d":"0.89"},{"v":0.8867640806305532,"d":"0.89"},{"v":0.094606337,"d":"0.09"}]
["22081","Red River","LA",{"v":0.7999400773488928,"d":"0.80"},{"v":0.7999400773488928,"d":"0.80"},{"v":0.113884937,"d":"0.11"}]
["22083","Richland","LA",{"v":0.916928747117725,"d":"0.92"},{"v":0.916928747117725,"d":"0.92"},{"v":0.076404662,"d":"0.08"}]
["22085","Sabine","LA",{"v":0.869585231410212,"d":"0.87"},{"v":0.8695852314102122,"d":"0.87"},{"v":0.132249996,"d":"0.13"}]
["22087","St Bernard","LA",{"v":0.7288949986962552,"d":"0.73"},{"v":0.7288949986962553,"d":"0.73"},{"v":0.024090344,"d":"0.02"}]
["22089","St Charles","LA",{"v":0.7706148127053952,"d":"0.77"},{"v":0.7706148127053953,"d":"0.77"},{"v":0.036324775,"d":"0.04"}]
["22091","St Helena","LA",{"v":0.87422617289245,"d":"0.87"},{"v":0.87422617289245,"d":"0.87"},{"v":0.141052426,"d":"0.14"}]
["22093","St James","LA",{"v":0.6588953727396838,"d":"0.66"},{"v":0.6588953727396837,"d":"0.66"},{"v":0.06015456,"d":"0.06"}]
["22095","St John The Baptist","LA",{"v":0.7948586706245476,"d":"0.79"},{"v":0.7948586706245475,"d":"0.79"},{"v":0.04995491500000001,"d":"0.05"}]
["22097","St Landry","LA",{"v":0.8200037128563127,"d":"0.82"},{"v":0.8200037128563127,"d":"0.82"},{"v":0.069815194,"d":"0.07"}]
["22099","St Martin","LA",{"v":0.7658572030558283,"d":"0.77"},{"v":0.7658572030558284,"d":"0.77"},{"v":0.089301683,"d":"0.09"}]
["22101","St Mary","LA",{"v":0.8067547912321421,"d":"0.81"},{"v":0.8067547912321421,"d":"0.81"},{"v":0.047167333,"d":"0.05"}]
["22103","St Tammany","LA",{"v":0.7893502648896084,"d":"0.79"},{"v":0.7893502648896081,"d":"0.79"},{"v":0.077356537,"d":"0.08"}]
["22105","Tangipahoa","LA",{"v":0.8162328477948068,"d":"0.82"},{"v":0.8162328477948068,"d":"0.82"},{"v":0.08787555,"d":"0.09"}]
["22107","Tensas","LA",{"v":0.7711061179411715,"d":"0.77"},{"v":0.7711061179411713,"d":"0.77"},{"v":0.081545722,"d":"0.08"}]
["22109","Terrebonne","LA",{"v":0.700636411136226,"d":"0.70"},{"v":0.700636411136226,"d":"0.70"},{"v":0.0332593,"d":"0.03"}]
["22111","Union","LA",{"v":0.8917830060126826,"d":"0.89"},{"v":0.8917830060126826,"d":"0.89"},{"v":0.147771108,"d":"0.15"}]
["22113","Vermilion","LA",{"v":0.8279226597843388,"d":"0.83"},{"v":0.8279226597843389,"d":"0.83"},{"v":0.04567573700000001,"d":"0.05"}]
["22115","Vernon","LA",{"v":0.8754579091213541,"d":"0.88"},{"v":0.8754579091213541,"d":"0.88"},{"v":0.128132836,"d":"0.13"}]
["22117","Washington","LA",{"v":0.799588035134594,"d":"0.80"},{"v":0.799588035134594,"d":"0.80"},{"v":0.101232534,"d":"0.10"}]
["22119","Webster","LA",{"v":0.8712721363945002,"d":"0.87"},{"v":0.8712721363945002,"d":"0.87"},{"v":0.109448248,"d":"0.11"}]
["22121","West Baton Rouge","LA",{"v":0.8038046076394468,"d":"0.80"},{"v":0.8038046076394467,"d":"0.80"},{"v":0.06780503,"d":"0.07"}]
["22123","West Carroll","LA",{"v":0.8046009277928479,"d":"0.80"},{"v":0.8046009277928478,"d":"0.80"},{"v":0.076569264,"d":"0.08"}]
["22125","West Feliciana","LA",{"v":0.7783258123971962,"d":"0.78"},{"v":0.7783258123971962,"d":"0.78"},{"v":0.118507236,"d":"0.12"}]
["22127","Winn","LA",{"v":0.9088882907280852,"d":"0.91"},{"v":0.9088882907280851,"d":"0.91"},{"v":0.152725339,"d":"0.15"}]
["23001","Androscoggin","ME",{"v":4.93456758117587,"d":"4.93"},{"v":4.934567581175869,"d":"4.93"},{"v":2.93053264,"d":"2.93"}]
["23003","Aroostook","ME",{"v":5.7785202124589645,"d":"5.78"},{"v":5.7785202124589645,"d":"5.78"},{"v":5.328436023,"d":"5.33"}]
["23005","Cumberland","ME",{"v":4.8831011173483265,"d":"4.88"},{"v":4.883101117348326,"d":"4.88"},{"v":2.007868731,"d":"2.01"}]
["23007","Franklin","ME",{"v":5.988721289600248,"d":"5.99"},{"v":5.988721289600249,"d":"5.99"},{"v":5.970825941,"d":"5.97"}]
["23009","Hancock","ME",{"v":5.149844481870755,"d":"5.15"},{"v":5.149844481870755,"d":"5.15"},{"v":2.362622471,"d":"2.36"}]
["23011","Kennebec","ME",{"v":5.240908180014363,"d":"5.24"},{"v":5.240908180014363,"d":"5.24"},{"v":3.143409736,"d":"3.14"}]
["23013","Knox","ME",{"v":4.848081975802701,"d":"4.85"},{"v":4.848081975802701,"d":"4.85"},{"v":1.675636474,"d":"1.68"}]
["23015","Lincoln","ME",{"v":5.1524024184009605,"d":"5.15"},{"v":5.1524024184009605,"d":"5.15"},{"v":2.342851571,"d":"2.34"}]
["23017","Oxford","ME",{"v":5.91197679952127,"d":"5.91"},{"v":5.911976799521269,"d":"5.91"},{"v":5.911527918,"d":"5.91"}]
["23019","Penobscot","ME",{"v":5.298432146245122,"d":"5.30"},{"v":5.298432146245122,"d":"5.30"},{"v":3.072027547,"d":"3.07"}]
["23021","Piscataquis","ME",{"v":5.891289706078462,"d":"5.89"},{"v":5.891289706078464,"d":"5.89"},{"v":5.559924478,"d":"5.56"}]
["23023","Sagadahoc","ME",{"v":5.013561360267291,"d":"5.01"},{"v":5.013561360267291,"d":"5.01"},{"v":2.140536193,"d":"2.14"}]
["23025","Somerset","ME",{"v":5.844238944112454,"d":"5.84"},{"v":5.844238944112454,"d":"5.84"},{"v":5.531322422,"d":"5.53"}]
["23027","Waldo","ME",{"v":5.115309462413765,"d":"5.12"},{"v":5.115309462413764,"d":"5.12"},{"v":2.888376394,"d":"2.89"}]
["23029","Washington","ME",{"v":5.414469672889132,"d":"5.41"},{"v":5.414469672889132,"d":"5.41"},{"v":3.015862753,"d":"3.02"}]
["23031","York","ME",{"v":4.997668744119293,"d":"5.00"},{"v":4.997668744119293,"d":"5.00"},{"v":2.503375813,"d":"2.50"}]
["24001","Allegany","MD",{"v":3.6227744256658507,"d":"3.62"},{"v":3.6227744256658507,"d":"3.62"},{"v":0.9195410759999999,"d":"0.92"}]
["24003","Anne Arundel","MD",{"v":1.8017283872903855,"d":"1.80"},{"v":1.8017283872903855,"d":"1.80"},{"v":0.806952199,"d":"0.81"}]
["24005","Baltimore","MD",{"v":1.5760467500888564,"d":"1.58"},{"v":1.5760467500888564,"d":"1.58"},{"v":0.846499335,"d":"0.85"}]
["24009","Calvert","MD",{"v":3.3322095393766036,"d":"3.33"},{"v":3.3322095393766036,"d":"3.33"},{"v":0.628792031,"d":"0.63"}]
["24011","Caroline","MD",{"v":3.5592416940440157,"d":"3.56"},{"v":3.5592416940440157,"d":"3.56"},{"v":0.625072778,"d":"0.63"}]
["24013","Carroll","MD",{"v":3.7339890412303833,"d":"3.73"},{"v":3.7339890412303838,"d":"3.73"},{"v":0.688639122,"d":"0.69"}]
["24015","Cecil","MD",{"v":3.4040078128860434,"d":"3.40"},{"v":3.4040078128860434,"d":"3.40"},{"v":0.694080078,"d":"0.69"}]
["24017","Charles","MD",{"v":3.688481864740481,"d":"3.69"},{"v":3.688481864740481,"d":"3.69"},{"v":0.644534457,"d":"0.64"}]
["24019","Dorchester","MD",{"v":3.493283167489565,"d":"3.49"},{"v":3.4932831674895644,"d":"3.49"},{"v":0.453564537,"d":"0.45"}]
["24021","Frederick","MD",{"v":3.9608118720604364,"d":"3.96"},{"v":3.960811872060436,"d":"3.96"},{"v":0.635756792,"d":"0.64"}]
["24023","Garrett","MD",{"v":4.215491111692147,"d":"4.22"},{"v":4.215491111692146,"d":"4.22"},{"v":1.694234798,"d":"1.69"}]
["24025","Harford","MD",{"v":3.462334900026919,"d":"3.46"},{"v":3.462334900026919,"d":"3.46"},{"v":0.61093783,"d":"0.61"}]
["24027","Howard","MD",{"v":2.281174949764872,"d":"2.28"},{"v":2.281174949764872,"d":"2.28"},{"v":0.902149362,"d":"0.90"}]
["24029","Kent","MD",{"v":3.8087717634440423,"d":"3.81"},{"v":3.8087717634440423,"d":"3.81"},{"v":0.56341793,"d":"0.56"}]
["24031","Montgomery","MD",{"v":0.2515074150375197,"d":"0.25"},{"v":0.2515074150375197,"d":"0.25"},{"v":1.279524959,"d":"1.28"}]
["24033","Prince Georges","MD",{"v":0.731400684462528,"d":"0.73"},{"v":0.731400684462528,"d":"0.73"},{"v":1.029496098,"d":"1.03"}]
["24035","Queen Annes","MD",{"v":3.8320312908000744,"d":"3.83"},{"v":3.832031290800074,"d":"3.83"},{"v":0.571022741,"d":"0.57"}]
["24037","St Marys","MD",{"v":3.555175357875856,"d":"3.56"},{"v":3.555175357875856,"d":"3.56"},{"v":0.616265583,"d":"0.62"}]
["24039","Somerset","MD",{"v":3.415844122338779,"d":"3.42"},{"v":3.4158441223387794,"d":"3.42"},{"v":0.471674827,"d":"0.47"}]
["24041","Talbot","MD",{"v":3.41012481563469,"d":"3.41"},{"v":3.4101248156346906,"d":"3.41"},{"v":0.443077718,"d":"0.44"}]
["24043","Washington","MD",{"v":4.287128617610081,"d":"4.29"},{"v":4.2871286176100805,"d":"4.29"},{"v":0.8291595929999999,"d":"0.83"}]
["24045","Wicomico","MD",{"v":3.420148834495669,"d":"3.42"},{"v":3.4201488344956688,"d":"3.42"},{"v":0.513520224,"d":"0.51"}]
["24047","Worcester","MD",{"v":3.484713653889791,"d":"3.48"},{"v":3.484713653889791,"d":"3.48"},{"v":0.469913943,"d":"0.47"}]
["24510","Baltimore City","MD",{"v":5.7866805968427506E-11,"d":"0.00"},{"v":5.7866805968427506E-11,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["25001","Barnstable","MA",{"v":2.6204938823622568,"d":"2.62"},{"v":2.6204938823622568,"d":"2.62"},{"v":0.362921498,"d":"0.36"}]
["25003","Berkshire","MA",{"v":3.054145639154131,"d":"3.05"},{"v":3.0541456391541315,"d":"3.05"},{"v":1.252666421,"d":"1.25"}]
["25005","Bristol","MA",{"v":1.6011598462653391,"d":"1.60"},{"v":1.6011598462653391,"d":"1.60"},{"v":0.750873493,"d":"0.75"}]
["25007","Dukes","MA",{"v":2.7010456315475158,"d":"2.70"},{"v":2.7010456315475153,"d":"2.70"},{"v":0.468384302,"d":"0.47"}]
["25009","Essex","MA",{"v":0.598246565638993,"d":"0.60"},{"v":0.598246565638993,"d":"0.60"},{"v":0.814019344,"d":"0.81"}]
["25011","Franklin","MA",{"v":3.0248070903463717,"d":"3.02"},{"v":3.024807090346372,"d":"3.02"},{"v":1.259687168,"d":"1.26"}]
["25013","Hampden","MA",{"v":2.394642969217853,"d":"2.39"},{"v":2.3946429692178524,"d":"2.39"},{"v":0.990186097,"d":"0.99"}]
["25015","Hampshire","MA",{"v":2.734406784334571,"d":"2.73"},{"v":2.734406784334571,"d":"2.73"},{"v":1.074526648,"d":"1.07"}]
["25017","Middlesex","MA",{"v":0.21762573609889144,"d":"0.22"},{"v":0.2176257360988914,"d":"0.22"},{"v":1.517841025,"d":"1.52"}]
["25019","Nantucket","MA",{"v":2.87884820161907,"d":"2.88"},{"v":2.8788482016190704,"d":"2.88"},{"v":0.410001363,"d":"0.41"}]
["25021","Norfolk","MA",{"v":0.31536732807557816,"d":"0.32"},{"v":0.3153673280755781,"d":"0.32"},{"v":1.32467197,"d":"1.32"}]
["25023","Plymouth","MA",{"v":1.7699985474445554,"d":"1.77"},{"v":1.7699985474445552,"d":"1.77"},{"v":0.586760702,"d":"0.59"}]
["25025","Suffolk","MA",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["25027","Worcester","MA",{"v":2.634874967305395,"d":"2.63"},{"v":2.634874967305395,"d":"2.63"},{"v":1.038814601,"d":"1.04"}]
["26001","Alcona","MI",{"v":2.665474186669335,"d":"2.67"},{"v":2.6654741866693357,"d":"2.67"},{"v":1.324626685,"d":"1.32"}]
["26003","Alger","MI",{"v":3.248087811095464,"d":"3.25"},{"v":3.2480878110954645,"d":"3.25"},{"v":1.608274272,"d":"1.61"}]
["26005","Allegan","MI",{"v":2.607650925846199,"d":"2.61"},{"v":2.6076509258461984,"d":"2.61"},{"v":0.510394914,"d":"0.51"}]
["26007","Alpena","MI",{"v":2.4333056960488695,"d":"2.43"},{"v":2.43330569604887,"d":"2.43"},{"v":0.764055841,"d":"0.76"}]
["26009","Antrim","MI",{"v":2.7197108870303914,"d":"2.72"},{"v":2.719710887030392,"d":"2.72"},{"v":1.056353423,"d":"1.06"}]
["26011","Arenac","MI",{"v":2.678244598792246,"d":"2.68"},{"v":2.6782445987922463,"d":"2.68"},{"v":0.714263317,"d":"0.71"}]
["26013","Baraga","MI",{"v":3.3053925104785704,"d":"3.31"},{"v":3.30539251047857,"d":"3.31"},{"v":1.881025861,"d":"1.88"}]
["26015","Barry","MI",{"v":2.7699460994617953,"d":"2.77"},{"v":2.7699460994617953,"d":"2.77"},{"v":0.632372541,"d":"0.63"}]
["26017","Bay","MI",{"v":2.508760458255929,"d":"2.51"},{"v":2.5087604582559293,"d":"2.51"},{"v":0.407196856,"d":"0.41"}]
["26019","Benzie","MI",{"v":2.839785103279113,"d":"2.84"},{"v":2.839785103279113,"d":"2.84"},{"v":0.9967351510000001,"d":"1.00"}]
["26021","Berrien","MI",{"v":2.214689449376889,"d":"2.21"},{"v":2.214689449376889,"d":"2.21"},{"v":0.434415838,"d":"0.43"}]
["26023","Branch","MI",{"v":2.6041152833848242,"d":"2.60"},{"v":2.6041152833848247,"d":"2.60"},{"v":0.489629258,"d":"0.49"}]
["26025","Calhoun","MI",{"v":2.7562619037308895,"d":"2.76"},{"v":2.756261903730889,"d":"2.76"},{"v":0.421864739,"d":"0.42"}]
["26027","Cass","MI",{"v":2.5646647880056177,"d":"2.56"},{"v":2.5646647880056177,"d":"2.56"},{"v":0.545704776,"d":"0.55"}]
["26029","Charlevoix","MI",{"v":2.7010939439593966,"d":"2.70"},{"v":2.7010939439593966,"d":"2.70"},{"v":0.718261466,"d":"0.72"}]
["26031","Cheboygan","MI",{"v":2.6102023191373687,"d":"2.61"},{"v":2.6102023191373687,"d":"2.61"},{"v":1.02170344,"d":"1.02"}]
["26033","Chippewa","MI",{"v":2.792887624618126,"d":"2.79"},{"v":2.792887624618126,"d":"2.79"},{"v":1.198402518,"d":"1.20"}]
["26035","Clare","MI",{"v":2.8296100250812817,"d":"2.83"},{"v":2.8296100250812817,"d":"2.83"},{"v":0.965369569,"d":"0.97"}]
["26037","Clinton","MI",{"v":2.4503266653510587,"d":"2.45"},{"v":2.4503266653510587,"d":"2.45"},{"v":0.432459972,"d":"0.43"}]
["26039","Crawford","MI",{"v":2.950090125503531,"d":"2.95"},{"v":2.9500901255035314,"d":"2.95"},{"v":1.325165948,"d":"1.33"}]
["26041","Delta","MI",{"v":2.891465166229964,"d":"2.89"},{"v":2.891465166229964,"d":"2.89"},{"v":1.055330969,"d":"1.06"}]
["26043","Dickinson","MI",{"v":2.7821950897713656,"d":"2.78"},{"v":2.7821950897713656,"d":"2.78"},{"v":1.4519671250000001,"d":"1.45"}]
["26045","Eaton","MI",{"v":2.4472125954607407,"d":"2.45"},{"v":2.447212595460741,"d":"2.45"},{"v":0.43290465,"d":"0.43"}]
["26047","Emmet","MI",{"v":2.6930987209578294,"d":"2.69"},{"v":2.693098720957829,"d":"2.69"},{"v":0.852390715,"d":"0.85"}]
["26049","Genesee","MI",{"v":2.239133310665479,"d":"2.24"},{"v":2.239133310665479,"d":"2.24"},{"v":0.446442081,"d":"0.45"}]
["26051","Gladwin","MI",{"v":2.803859362936831,"d":"2.80"},{"v":2.8038593629368305,"d":"2.80"},{"v":0.916949271,"d":"0.92"}]
["26053","Gogebic","MI",{"v":3.347232819281018,"d":"3.35"},{"v":3.3472328192810186,"d":"3.35"},{"v":1.768875242,"d":"1.77"}]
["26055","Grand Traverse","MI",{"v":2.6790153377032486,"d":"2.68"},{"v":2.679015337703248,"d":"2.68"},{"v":0.757371086,"d":"0.76"}]
["26057","Gratiot","MI",{"v":2.8819823355967524,"d":"2.88"},{"v":2.8819823355967524,"d":"2.88"},{"v":0.541299192,"d":"0.54"}]
["26059","Hillsdale","MI",{"v":2.042527395691977,"d":"2.04"},{"v":2.042527395691977,"d":"2.04"},{"v":0.541200932,"d":"0.54"}]
["26061","Houghton","MI",{"v":3.298151424631954,"d":"3.30"},{"v":3.2981514246319543,"d":"3.30"},{"v":1.438889634,"d":"1.44"}]
["26063","Huron","MI",{"v":2.885634602245167,"d":"2.89"},{"v":2.885634602245167,"d":"2.89"},{"v":0.489395628,"d":"0.49"}]
["26065","Ingham","MI",{"v":2.371544707606671,"d":"2.37"},{"v":2.3715447076066716,"d":"2.37"},{"v":0.426022726,"d":"0.43"}]
["26067","Ionia","MI",{"v":2.6358548441063516,"d":"2.64"},{"v":2.6358548441063516,"d":"2.64"},{"v":0.524042712,"d":"0.52"}]
["26069","Iosco","MI",{"v":2.7850713477302365,"d":"2.79"},{"v":2.785071347730237,"d":"2.79"},{"v":0.802908961,"d":"0.80"}]
["26071","Iron","MI",{"v":3.2903692052080875,"d":"3.29"},{"v":3.290369205208088,"d":"3.29"},{"v":1.800520302,"d":"1.80"}]
["26073","Isabella","MI",{"v":2.6868248138653583,"d":"2.69"},{"v":2.6868248138653583,"d":"2.69"},{"v":0.62794015,"d":"0.63"}]
["26075","Jackson","MI",{"v":2.4201723813856955,"d":"2.42"},{"v":2.420172381385696,"d":"2.42"},{"v":0.49027543800000006,"d":"0.49"}]
["26077","Kalamazoo","MI",{"v":2.382445295443007,"d":"2.38"},{"v":2.382445295443007,"d":"2.38"},{"v":0.44782810500000003,"d":"0.45"}]
["26079","Kalkaska","MI",{"v":2.824986527354256,"d":"2.82"},{"v":2.8249865273542567,"d":"2.82"},{"v":1.259455515,"d":"1.26"}]
["26081","Kent","MI",{"v":2.177933825419681,"d":"2.18"},{"v":2.177933825419681,"d":"2.18"},{"v":0.513070033,"d":"0.51"}]
["26083","Keweenaw","MI",{"v":3.280192308486142,"d":"3.28"},{"v":3.280192308486142,"d":"3.28"},{"v":1.269801131,"d":"1.27"}]
["26085","Lake","MI",{"v":2.999894009627178,"d":"3.00"},{"v":2.999894009627178,"d":"3.00"},{"v":1.395130229,"d":"1.40"}]
["26087","Lapeer","MI",{"v":2.482083405085346,"d":"2.48"},{"v":2.482083405085346,"d":"2.48"},{"v":0.537649009,"d":"0.54"}]
["26089","Leelanau","MI",{"v":2.8238142672833995,"d":"2.82"},{"v":2.8238142672833995,"d":"2.82"},{"v":0.704242452,"d":"0.70"}]
["26091","Lenawee","MI",{"v":2.4306977547030826,"d":"2.43"},{"v":2.4306977547030826,"d":"2.43"},{"v":0.381258319,"d":"0.38"}]
["26093","Livingston","MI",{"v":2.5222980451428367,"d":"2.52"},{"v":2.5222980451428367,"d":"2.52"},{"v":0.48043564800000005,"d":"0.48"}]
["26095","Luce","MI",{"v":2.6408152856843494,"d":"2.64"},{"v":2.64081528568435,"d":"2.64"},{"v":1.466639095,"d":"1.47"}]
["26097","Mackinac","MI",{"v":3.1644091473282394,"d":"3.16"},{"v":3.1644091473282394,"d":"3.16"},{"v":1.409490543,"d":"1.41"}]
["26099","Macomb","MI",{"v":0.2606968167393721,"d":"0.26"},{"v":0.2606968167393722,"d":"0.26"},{"v":0.634370774,"d":"0.63"}]
["26101","Manistee","MI",{"v":2.6973344867011066,"d":"2.70"},{"v":2.697334486701107,"d":"2.70"},{"v":0.909710211,"d":"0.91"}]
["26103","Marquette","MI",{"v":3.1575031466422745,"d":"3.16"},{"v":3.1575031466422745,"d":"3.16"},{"v":1.37038417,"d":"1.37"}]
["26105","Mason","MI",{"v":2.6331630830553574,"d":"2.63"},{"v":2.633163083055358,"d":"2.63"},{"v":0.689128571,"d":"0.69"}]
["26107","Mecosta","MI",{"v":2.7477404804583507,"d":"2.75"},{"v":2.7477404804583507,"d":"2.75"},{"v":0.812323255,"d":"0.81"}]
["26109","Menominee","MI",{"v":3.2701308973085808,"d":"3.27"},{"v":3.2701308973085808,"d":"3.27"},{"v":1.612864971,"d":"1.61"}]
["26111","Midland","MI",{"v":2.6498661731125397,"d":"2.65"},{"v":2.6498661731125397,"d":"2.65"},{"v":0.657061438,"d":"0.66"}]
["26113","Missaukee","MI",{"v":2.983185547861289,"d":"2.98"},{"v":2.9831855478612894,"d":"2.98"},{"v":1.257906481,"d":"1.26"}]
["26115","Monroe","MI",{"v":2.439335989800528,"d":"2.44"},{"v":2.439335989800528,"d":"2.44"},{"v":0.351130697,"d":"0.35"}]
["26117","Montcalm","MI",{"v":2.834995415170543,"d":"2.83"},{"v":2.8349954151705425,"d":"2.83"},{"v":0.747618224,"d":"0.75"}]
["26119","Montmorency","MI",{"v":2.592961032028944,"d":"2.59"},{"v":2.5929610320289442,"d":"2.59"},{"v":1.373405638,"d":"1.37"}]
["26121","Muskegon","MI",{"v":2.6399968146208828,"d":"2.64"},{"v":2.6399968146208828,"d":"2.64"},{"v":0.54657118,"d":"0.55"}]
["26123","Newaygo","MI",{"v":2.860170072664999,"d":"2.86"},{"v":2.8601700726649995,"d":"2.86"},{"v":1.054934083,"d":"1.05"}]
["26125","Oakland","MI",{"v":0.7609163349355684,"d":"0.76"},{"v":0.7609163349355684,"d":"0.76"},{"v":0.664883854,"d":"0.66"}]
["26127","Oceana","MI",{"v":2.8038107236299186,"d":"2.80"},{"v":2.803810723629918,"d":"2.80"},{"v":0.878742336,"d":"0.88"}]
["26129","Ogemaw","MI",{"v":2.9442664438424173,"d":"2.94"},{"v":2.9442664438424173,"d":"2.94"},{"v":1.319332456,"d":"1.32"}]
["26131","Ontonagon","MI",{"v":3.418407372693703,"d":"3.42"},{"v":3.4184073726937036,"d":"3.42"},{"v":2.059453166,"d":"2.06"}]
["26133","Osceola","MI",{"v":2.5823018043874195,"d":"2.58"},{"v":2.5823018043874195,"d":"2.58"},{"v":1.025107684,"d":"1.03"}]
["26135","Oscoda","MI",{"v":2.8623873077268307,"d":"2.86"},{"v":2.8623873077268307,"d":"2.86"},{"v":1.536592731,"d":"1.54"}]
["26137","Otsego","MI",{"v":2.6062505553815036,"d":"2.61"},{"v":2.6062505553815036,"d":"2.61"},{"v":1.123673488,"d":"1.12"}]
["26139","Ottawa","MI",{"v":2.3259635650546118,"d":"2.33"},{"v":2.3259635650546118,"d":"2.33"},{"v":0.394891839,"d":"0.39"}]
["26141","Presque Isle","MI",{"v":2.5405814203341226,"d":"2.54"},{"v":2.540581420334123,"d":"2.54"},{"v":0.943765105,"d":"0.94"}]
["26143","Roscommon","MI",{"v":2.800103073591298,"d":"2.80"},{"v":2.8001030735912975,"d":"2.80"},{"v":0.986471255,"d":"0.99"}]
["26145","Saginaw","MI",{"v":2.289792274100897,"d":"2.29"},{"v":2.289792274100897,"d":"2.29"},{"v":0.447460072,"d":"0.45"}]
["26147","St Clair","MI",{"v":2.4630482702046725,"d":"2.46"},{"v":2.4630482702046725,"d":"2.46"},{"v":0.374803752,"d":"0.37"}]
["26149","St Joseph","MI",{"v":2.8320319076036173,"d":"2.83"},{"v":2.8320319076036173,"d":"2.83"},{"v":0.448261646,"d":"0.45"}]
["26151","Sanilac","MI",{"v":2.77631638368275,"d":"2.78"},{"v":2.77631638368275,"d":"2.78"},{"v":0.559378411,"d":"0.56"}]
["26153","Schoolcraft","MI",{"v":3.0916809089597628,"d":"3.09"},{"v":3.0916809089597628,"d":"3.09"},{"v":1.329276811,"d":"1.33"}]
["26155","Shiawassee","MI",{"v":2.4003306772838124,"d":"2.40"},{"v":2.4003306772838124,"d":"2.40"},{"v":0.447790517,"d":"0.45"}]
["26157","Tuscola","MI",{"v":2.6919026896870615,"d":"2.69"},{"v":2.691902689687062,"d":"2.69"},{"v":0.621334512,"d":"0.62"}]
["26159","Van Buren","MI",{"v":2.602827386420555,"d":"2.60"},{"v":2.6028273864205547,"d":"2.60"},{"v":0.567013536,"d":"0.57"}]
["26161","Washtenaw","MI",{"v":2.3875222464427326,"d":"2.39"},{"v":2.387522246442733,"d":"2.39"},{"v":0.431019685,"d":"0.43"}]
["26163","Wayne","MI",{"v":5.79328734557359E-3,"d":"0.01"},{"v":5.79328734557359E-3,"d":"0.01"},{"v":1.170037947,"d":"1.17"}]
["26165","Wexford","MI",{"v":2.7744639870985277,"d":"2.77"},{"v":2.7744639870985277,"d":"2.77"},{"v":1.086904706,"d":"1.09"}]
["27001","Aitkin","MN",{"v":2.8606264917304483,"d":"2.86"},{"v":2.860626491730448,"d":"2.86"},{"v":1.670739332,"d":"1.67"}]
["27003","Anoka","MN",{"v":2.6822967304645307,"d":"2.68"},{"v":2.682296730464531,"d":"2.68"},{"v":0.8998719979999998,"d":"0.90"}]
["27005","Becker","MN",{"v":3.168489778136878,"d":"3.17"},{"v":3.1684897781368777,"d":"3.17"},{"v":1.466175656,"d":"1.47"}]
["27007","Beltrami","MN",{"v":2.946138556984495,"d":"2.95"},{"v":2.946138556984495,"d":"2.95"},{"v":1.427681842,"d":"1.43"}]
["27009","Benton","MN",{"v":2.9036034128627572,"d":"2.90"},{"v":2.903603412862757,"d":"2.90"},{"v":0.715654014,"d":"0.72"}]
["27011","Big Stone","MN",{"v":3.0768580279311024,"d":"3.08"},{"v":3.0768580279311024,"d":"3.08"},{"v":0.939710222,"d":"0.94"}]
["27013","Blue Earth","MN",{"v":2.8038291231306167,"d":"2.80"},{"v":2.8038291231306167,"d":"2.80"},{"v":0.509714761,"d":"0.51"}]
["27015","Brown","MN",{"v":2.832881354553695,"d":"2.83"},{"v":2.8328813545536953,"d":"2.83"},{"v":0.525587881,"d":"0.53"}]
["27017","Carlton","MN",{"v":2.812224263427393,"d":"2.81"},{"v":2.812224263427393,"d":"2.81"},{"v":1.322682039,"d":"1.32"}]
["27019","Carver","MN",{"v":2.669609009192662,"d":"2.67"},{"v":2.6696090091926625,"d":"2.67"},{"v":0.595314565,"d":"0.60"}]
["27021","Cass","MN",{"v":3.114165277879731,"d":"3.11"},{"v":3.1141652778797306,"d":"3.11"},{"v":1.897693129,"d":"1.90"}]
["27023","Chippewa","MN",{"v":2.908801962708772,"d":"2.91"},{"v":2.9088019627087722,"d":"2.91"},{"v":0.682698705,"d":"0.68"}]
["27025","Chisago","MN",{"v":3.1682316608913923,"d":"3.17"},{"v":3.168231660891392,"d":"3.17"},{"v":0.904211984,"d":"0.90"}]
["27027","Clay","MN",{"v":3.1952319846901465,"d":"3.20"},{"v":3.195231984690146,"d":"3.20"},{"v":0.863949231,"d":"0.86"}]
["27029","Clearwater","MN",{"v":3.257770806285011,"d":"3.26"},{"v":3.257770806285011,"d":"3.26"},{"v":1.777184449,"d":"1.78"}]
["27031","Cook","MN",{"v":3.1037105117105988,"d":"3.10"},{"v":3.1037105117105983,"d":"3.10"},{"v":2.548887857,"d":"2.55"}]
["27033","Cottonwood","MN",{"v":2.884967963907014,"d":"2.88"},{"v":2.884967963907014,"d":"2.88"},{"v":0.624227989,"d":"0.62"}]
["27035","Crow Wing","MN",{"v":2.890214440036852,"d":"2.89"},{"v":2.8902144400368526,"d":"2.89"},{"v":1.049396162,"d":"1.05"}]
["27037","Dakota","MN",{"v":2.428933937004176,"d":"2.43"},{"v":2.428933937004176,"d":"2.43"},{"v":0.569359967,"d":"0.57"}]
["27039","Dodge","MN",{"v":2.8978607546556905,"d":"2.90"},{"v":2.89786075465569,"d":"2.90"},{"v":0.571265424,"d":"0.57"}]
["27041","Douglas","MN",{"v":2.5864057255676807,"d":"2.59"},{"v":2.5864057255676816,"d":"2.59"},{"v":0.828835215,"d":"0.83"}]
["27043","Faribault","MN",{"v":2.894009500370193,"d":"2.89"},{"v":2.894009500370193,"d":"2.89"},{"v":0.68782225,"d":"0.69"}]
["27045","Fillmore","MN",{"v":2.8271503698691975,"d":"2.83"},{"v":2.8271503698691975,"d":"2.83"},{"v":0.828962385,"d":"0.83"}]
["27047","Freeborn","MN",{"v":2.816507599870227,"d":"2.82"},{"v":2.8165075998702265,"d":"2.82"},{"v":0.542752654,"d":"0.54"}]
["27049","Goodhue","MN",{"v":2.8018742650284976,"d":"2.80"},{"v":2.801874265028497,"d":"2.80"},{"v":0.629612519,"d":"0.63"}]
["27051","Grant","MN",{"v":3.0251474450590967,"d":"3.03"},{"v":3.0251474450590963,"d":"3.03"},{"v":1.126060336,"d":"1.13"}]
["27053","Hennepin","MN",{"v":0.051171952243044445,"d":"0.05"},{"v":0.051171952243044445,"d":"0.05"},{"v":1.751277391,"d":"1.75"}]
["27055","Houston","MN",{"v":2.940135318032429,"d":"2.94"},{"v":2.940135318032429,"d":"2.94"},{"v":0.8774333030000001,"d":"0.88"}]
["27057","Hubbard","MN",{"v":2.8175160186268178,"d":"2.82"},{"v":2.8175160186268173,"d":"2.82"},{"v":1.8088892010000002,"d":"1.81"}]
["27059","Isanti","MN",{"v":3.291301450325778,"d":"3.29"},{"v":3.291301450325778,"d":"3.29"},{"v":1.030826864,"d":"1.03"}]
["27061","Itasca","MN",{"v":2.881286851585005,"d":"2.88"},{"v":2.881286851585004,"d":"2.88"},{"v":1.680761369,"d":"1.68"}]
["27063","Jackson","MN",{"v":2.9199587047647366,"d":"2.92"},{"v":2.9199587047647366,"d":"2.92"},{"v":0.673484273,"d":"0.67"}]
["27065","Kanabec","MN",{"v":3.161460526074442,"d":"3.16"},{"v":3.1614605260744417,"d":"3.16"},{"v":1.450222483,"d":"1.45"}]
["27067","Kandiyohi","MN",{"v":2.918375266118002,"d":"2.92"},{"v":2.918375266118002,"d":"2.92"},{"v":0.695446345,"d":"0.70"}]
["27069","Kittson","MN",{"v":3.1654983082872943,"d":"3.17"},{"v":3.165498308287294,"d":"3.17"},{"v":1.343477416,"d":"1.34"}]
["27071","Koochiching","MN",{"v":2.885667308795266,"d":"2.89"},{"v":2.885667308795266,"d":"2.89"},{"v":1.512321864,"d":"1.51"}]
["27073","Lac Qui Parle","MN",{"v":2.9839658515993617,"d":"2.98"},{"v":2.9839658515993617,"d":"2.98"},{"v":0.8702263800000001,"d":"0.87"}]
["27075","Lake","MN",{"v":2.925796570662739,"d":"2.93"},{"v":2.925796570662739,"d":"2.93"},{"v":1.811476766,"d":"1.81"}]
["27077","Lake of The Woods","MN",{"v":3.0052125505413736,"d":"3.01"},{"v":3.0052125505413736,"d":"3.01"},{"v":1.661705824,"d":"1.66"}]
["27079","Le Sueur","MN",{"v":2.878538367707578,"d":"2.88"},{"v":2.878538367707578,"d":"2.88"},{"v":0.636674742,"d":"0.64"}]
["27081","Lincoln","MN",{"v":3.0688213364087287,"d":"3.07"},{"v":3.0688213364087282,"d":"3.07"},{"v":0.830819824,"d":"0.83"}]
["27083","Lyon","MN",{"v":2.911473485707954,"d":"2.91"},{"v":2.911473485707954,"d":"2.91"},{"v":0.680324988,"d":"0.68"}]
["27085","McLeod","MN",{"v":3.109630033883523,"d":"3.11"},{"v":3.1096300338835237,"d":"3.11"},{"v":0.64226068,"d":"0.64"}]
["27087","Mahnomen","MN",{"v":2.912197706486433,"d":"2.91"},{"v":2.9121977064864333,"d":"2.91"},{"v":1.6870759280000003,"d":"1.69"}]
["27089","Marshall","MN",{"v":3.1575941484037844,"d":"3.16"},{"v":3.157594148403785,"d":"3.16"},{"v":1.341127143,"d":"1.34"}]
["27091","Martin","MN",{"v":2.874068609580139,"d":"2.87"},{"v":2.874068609580139,"d":"2.87"},{"v":0.567189141,"d":"0.57"}]
["27093","Meeker","MN",{"v":2.9913186511767718,"d":"2.99"},{"v":2.991318651176772,"d":"2.99"},{"v":0.8141099700000001,"d":"0.81"}]
["27095","Mille Lacs","MN",{"v":2.89379742746903,"d":"2.89"},{"v":2.89379742746903,"d":"2.89"},{"v":1.17663447,"d":"1.18"}]
["27097","Morrison","MN",{"v":3.182887677388177,"d":"3.18"},{"v":3.1828876773881776,"d":"3.18"},{"v":0.9977766260000002,"d":"1.00"}]
["27099","Mower","MN",{"v":2.7860752092321546,"d":"2.79"},{"v":2.786075209232155,"d":"2.79"},{"v":0.493177791,"d":"0.49"}]
["27101","Murray","MN",{"v":2.9655824875297037,"d":"2.97"},{"v":2.965582487529704,"d":"2.97"},{"v":0.861604203,"d":"0.86"}]
["27103","Nicollet","MN",{"v":2.8829633994827932,"d":"2.88"},{"v":2.8829633994827932,"d":"2.88"},{"v":0.512149603,"d":"0.51"}]
["27105","Nobles","MN",{"v":2.9069124223469123,"d":"2.91"},{"v":2.9069124223469127,"d":"2.91"},{"v":0.63112968,"d":"0.63"}]
["27107","Norman","MN",{"v":3.1356632399583972,"d":"3.14"},{"v":3.1356632399583977,"d":"3.14"},{"v":1.311027532,"d":"1.31"}]
["27109","Olmsted","MN",{"v":2.9024777146797387,"d":"2.90"},{"v":2.9024777146797387,"d":"2.90"},{"v":0.516818702,"d":"0.52"}]
["27111","Otter Tail","MN",{"v":3.170090675477382,"d":"3.17"},{"v":3.170090675477382,"d":"3.17"},{"v":0.982389089,"d":"0.98"}]
["27113","Pennington","MN",{"v":3.0620830256119946,"d":"3.06"},{"v":3.0620830256119946,"d":"3.06"},{"v":0.908268823,"d":"0.91"}]
["27115","Pine","MN",{"v":3.1098833261634207,"d":"3.11"},{"v":3.1098833261634202,"d":"3.11"},{"v":1.516398863,"d":"1.52"}]
["27117","Pipestone","MN",{"v":2.913521541382668,"d":"2.91"},{"v":2.913521541382668,"d":"2.91"},{"v":0.665032218,"d":"0.67"}]
["27119","Polk","MN",{"v":3.09476567122255,"d":"3.09"},{"v":3.0947656712225498,"d":"3.09"},{"v":1.009364911,"d":"1.01"}]
["27121","Pope","MN",{"v":2.1333448353018802,"d":"2.13"},{"v":2.1333448353018802,"d":"2.13"},{"v":0.903583981,"d":"0.90"}]
["27123","Ramsey","MN",{"v":4.3941188618566978E-4,"d":"0.00"},{"v":4.3941188618566978E-4,"d":"0.00"},{"v":3.746957738,"d":"3.75"}]
["27125","Red Lake","MN",{"v":2.978443002621933,"d":"2.98"},{"v":2.978443002621933,"d":"2.98"},{"v":1.487243791,"d":"1.49"}]
["27127","Redwood","MN",{"v":3.0999847402839213,"d":"3.10"},{"v":3.099984740283922,"d":"3.10"},{"v":0.735098278,"d":"0.74"}]
["27129","Renville","MN",{"v":2.9570125506519065,"d":"2.96"},{"v":2.9570125506519065,"d":"2.96"},{"v":0.808867861,"d":"0.81"}]
["27131","Rice","MN",{"v":2.647737642326945,"d":"2.65"},{"v":2.647737642326945,"d":"2.65"},{"v":0.558323576,"d":"0.56"}]
["27133","Rock","MN",{"v":2.8925205722931326,"d":"2.89"},{"v":2.892520572293132,"d":"2.89"},{"v":0.673633266,"d":"0.67"}]
["27135","Roseau","MN",{"v":2.5396152305936694,"d":"2.54"},{"v":2.5396152305936694,"d":"2.54"},{"v":1.396184053,"d":"1.40"}]
["27137","St Louis","MN",{"v":2.708814012690826,"d":"2.71"},{"v":2.708814012690826,"d":"2.71"},{"v":1.5116443839999998,"d":"1.51"}]
["27139","Scott","MN",{"v":2.847448064513195,"d":"2.85"},{"v":2.8474480645131957,"d":"2.85"},{"v":0.620155715,"d":"0.62"}]
["27141","Sherburne","MN",{"v":3.1424716423511447,"d":"3.14"},{"v":3.142471642351145,"d":"3.14"},{"v":0.757729534,"d":"0.76"}]
["27143","Sibley","MN",{"v":2.947419737814308,"d":"2.95"},{"v":2.9474197378143074,"d":"2.95"},{"v":0.818267502,"d":"0.82"}]
["27145","Stearns","MN",{"v":3.13646646658539,"d":"3.14"},{"v":3.1364664665853894,"d":"3.14"},{"v":0.70118148,"d":"0.70"}]
["27147","Steele","MN",{"v":2.838867519180539,"d":"2.84"},{"v":2.838867519180539,"d":"2.84"},{"v":0.503998596,"d":"0.50"}]
["27149","Stevens","MN",{"v":2.9266363215456064,"d":"2.93"},{"v":2.9266363215456064,"d":"2.93"},{"v":0.694402807,"d":"0.69"}]
["27151","Swift","MN",{"v":2.973247028666274,"d":"2.97"},{"v":2.9732470286662736,"d":"2.97"},{"v":0.793786549,"d":"0.79"}]
["27153","Todd","MN",{"v":3.0335979125682617,"d":"3.03"},{"v":3.033597912568262,"d":"3.03"},{"v":1.004865188,"d":"1.00"}]
["27155","Traverse","MN",{"v":3.0270224571009416,"d":"3.03"},{"v":3.0270224571009416,"d":"3.03"},{"v":1.087045852,"d":"1.09"}]
["27157","Wabasha","MN",{"v":3.0567467211253274,"d":"3.06"},{"v":3.056746721125328,"d":"3.06"},{"v":0.7909107600000002,"d":"0.79"}]
["27159","Wadena","MN",{"v":3.1182794545466326,"d":"3.12"},{"v":3.118279454546633,"d":"3.12"},{"v":0.959878459,"d":"0.96"}]
["27161","Waseca","MN",{"v":2.8754244312880006,"d":"2.88"},{"v":2.8754244312880006,"d":"2.88"},{"v":0.581630071,"d":"0.58"}]
["27163","Washington","MN",{"v":3.05107029625233,"d":"3.05"},{"v":3.05107029625233,"d":"3.05"},{"v":0.830431596,"d":"0.83"}]
["27165","Watonwan","MN",{"v":2.8334669174768363,"d":"2.83"},{"v":2.833466917476836,"d":"2.83"},{"v":0.601972779,"d":"0.60"}]
["27167","Wilkin","MN",{"v":2.9859010398092938,"d":"2.99"},{"v":2.985901039809294,"d":"2.99"},{"v":0.775196118,"d":"0.78"}]
["27169","Winona","MN",{"v":2.8691623573651066,"d":"2.87"},{"v":2.8691623573651066,"d":"2.87"},{"v":0.745235679,"d":"0.75"}]
["27171","Wright","MN",{"v":2.814531051158468,"d":"2.81"},{"v":2.8145310511584674,"d":"2.81"},{"v":0.6659842780000002,"d":"0.67"}]
["27173","Yellow Medicine","MN",{"v":2.9685689859604216,"d":"2.97"},{"v":2.9685689859604216,"d":"2.97"},{"v":0.8116309279999999,"d":"0.81"}]
["28001","Adams","MS",{"v":1.8263215117330802,"d":"1.83"},{"v":1.8263215117330802,"d":"1.83"},{"v":0.209413754,"d":"0.21"}]
["28003","Alcorn","MS",{"v":2.0994229903286636,"d":"2.10"},{"v":2.099422990328664,"d":"2.10"},{"v":0.345850366,"d":"0.35"}]
["28005","Amite","MS",{"v":2.163986636810965,"d":"2.16"},{"v":2.1639866368109653,"d":"2.16"},{"v":0.384225889,"d":"0.38"}]
["28007","Attala","MS",{"v":2.0154715871503894,"d":"2.02"},{"v":2.0154715871503894,"d":"2.02"},{"v":0.327755168,"d":"0.33"}]
["28009","Benton","MS",{"v":2.2249157084310265,"d":"2.22"},{"v":2.224915708431026,"d":"2.22"},{"v":0.384286256,"d":"0.38"}]
["28011","Bolivar","MS",{"v":1.8534738243061433,"d":"1.85"},{"v":1.853473824306143,"d":"1.85"},{"v":0.152464115,"d":"0.15"}]
["28013","Calhoun","MS",{"v":2.0325681078733138,"d":"2.03"},{"v":2.032568107873314,"d":"2.03"},{"v":0.378744493,"d":"0.38"}]
["28015","Carroll","MS",{"v":2.208477855483709,"d":"2.21"},{"v":2.2084778554837095,"d":"2.21"},{"v":0.382778547,"d":"0.38"}]
["28017","Chickasaw","MS",{"v":2.1218609876345846,"d":"2.12"},{"v":2.121860987634584,"d":"2.12"},{"v":0.284957548,"d":"0.28"}]
["28019","Choctaw","MS",{"v":2.0773738470367755,"d":"2.08"},{"v":2.0773738470367755,"d":"2.08"},{"v":0.416424042,"d":"0.42"}]
["28021","Claiborne","MS",{"v":2.190686565908094,"d":"2.19"},{"v":2.190686565908094,"d":"2.19"},{"v":0.352281937,"d":"0.35"}]
["28023","Clarke","MS",{"v":2.1608015465547217,"d":"2.16"},{"v":2.1608015465547217,"d":"2.16"},{"v":0.35658533,"d":"0.36"}]
["28025","Clay","MS",{"v":2.0713087013384284,"d":"2.07"},{"v":2.0713087013384284,"d":"2.07"},{"v":0.24639394,"d":"0.25"}]
["28027","Coahoma","MS",{"v":1.9116915992349326,"d":"1.91"},{"v":1.911691599234933,"d":"1.91"},{"v":0.137191349,"d":"0.14"}]
["28029","Copiah","MS",{"v":2.034409238880703,"d":"2.03"},{"v":2.034409238880703,"d":"2.03"},{"v":0.305023293,"d":"0.31"}]
["28031","Covington","MS",{"v":2.0031445049944963,"d":"2.00"},{"v":2.0031445049944963,"d":"2.00"},{"v":0.322167943,"d":"0.32"}]
["28033","De Soto","MS",{"v":2.052270884245195,"d":"2.05"},{"v":2.052270884245195,"d":"2.05"},{"v":0.19895764799999996,"d":"0.20"}]
["28035","Forrest","MS",{"v":2.0226043268060026,"d":"2.02"},{"v":2.0226043268060026,"d":"2.02"},{"v":0.23676614599999998,"d":"0.24"}]
["28037","Franklin","MS",{"v":2.1127353131692814,"d":"2.11"},{"v":2.112735313169282,"d":"2.11"},{"v":0.395025392,"d":"0.40"}]
["28039","George","MS",{"v":1.9376877996189439,"d":"1.94"},{"v":1.9376877996189439,"d":"1.94"},{"v":0.305377698,"d":"0.31"}]
["28041","Greene","MS",{"v":2.180713513775894,"d":"2.18"},{"v":2.180713513775894,"d":"2.18"},{"v":0.37969594,"d":"0.38"}]
["28043","Grenada","MS",{"v":2.0823565199517056,"d":"2.08"},{"v":2.082356519951706,"d":"2.08"},{"v":0.298400041,"d":"0.30"}]
["28045","Hancock","MS",{"v":2.0288867852178325,"d":"2.03"},{"v":2.028886785217833,"d":"2.03"},{"v":0.205100737,"d":"0.21"}]
["28047","Harrison","MS",{"v":1.9931712920134956,"d":"1.99"},{"v":1.9931712920134956,"d":"1.99"},{"v":0.161111343,"d":"0.16"}]
["28049","Hinds","MS",{"v":1.969466902761767,"d":"1.97"},{"v":1.9694669027617668,"d":"1.97"},{"v":0.188617666,"d":"0.19"}]
["28051","Holmes","MS",{"v":2.1424114121820734,"d":"2.14"},{"v":2.142411412182074,"d":"2.14"},{"v":0.284427735,"d":"0.28"}]
["28053","Humphreys","MS",{"v":1.7881751516041366,"d":"1.79"},{"v":1.7881751516041366,"d":"1.79"},{"v":0.132160609,"d":"0.13"}]
["28055","Issaquena","MS",{"v":2.066009944204895,"d":"2.07"},{"v":2.0660099442048954,"d":"2.07"},{"v":0.287253275,"d":"0.29"}]
["28057","Itawamba","MS",{"v":2.0810219732219957,"d":"2.08"},{"v":2.0810219732219957,"d":"2.08"},{"v":0.393662505,"d":"0.39"}]
["28059","Jackson","MS",{"v":1.959766240654741,"d":"1.96"},{"v":1.959766240654741,"d":"1.96"},{"v":0.164408487,"d":"0.16"}]
["28061","Jasper","MS",{"v":2.0950201073701886,"d":"2.10"},{"v":2.095020107370188,"d":"2.10"},{"v":0.375379264,"d":"0.38"}]
["28063","Jefferson","MS",{"v":2.0624790082718825,"d":"2.06"},{"v":2.0624790082718825,"d":"2.06"},{"v":0.36516933,"d":"0.37"}]
["28065","Jefferson Davis","MS",{"v":2.0973614882662623,"d":"2.10"},{"v":2.0973614882662623,"d":"2.10"},{"v":0.340838702,"d":"0.34"}]
["28067","Jones","MS",{"v":1.9951701487517755,"d":"2.00"},{"v":1.9951701487517757,"d":"2.00"},{"v":0.276810654,"d":"0.28"}]
["28069","Kemper","MS",{"v":2.0171924598272715,"d":"2.02"},{"v":2.017192459827272,"d":"2.02"},{"v":0.40129056,"d":"0.40"}]
["28071","Lafayette","MS",{"v":2.165947545030747,"d":"2.17"},{"v":2.165947545030747,"d":"2.17"},{"v":0.342017574,"d":"0.34"}]
["28073","Lamar","MS",{"v":1.8892215339408398,"d":"1.89"},{"v":1.8892215339408396,"d":"1.89"},{"v":0.282887303,"d":"0.28"}]
["28075","Lauderdale","MS",{"v":2.0154758515692537,"d":"2.02"},{"v":2.0154758515692537,"d":"2.02"},{"v":0.282366548,"d":"0.28"}]
["28077","Lawrence","MS",{"v":2.1205985462393486,"d":"2.12"},{"v":2.1205985462393486,"d":"2.12"},{"v":0.34858259,"d":"0.35"}]
["28079","Leake","MS",{"v":2.174746462937158,"d":"2.17"},{"v":2.174746462937158,"d":"2.17"},{"v":0.38978019,"d":"0.39"}]
["28081","Lee","MS",{"v":2.061658042855594,"d":"2.06"},{"v":2.061658042855594,"d":"2.06"},{"v":0.262738476,"d":"0.26"}]
["28083","Leflore","MS",{"v":1.9726580867770007,"d":"1.97"},{"v":1.9726580867770007,"d":"1.97"},{"v":0.10441789,"d":"0.10"}]
["28085","Lincoln","MS",{"v":2.045744820007261,"d":"2.05"},{"v":2.045744820007261,"d":"2.05"},{"v":0.303013454,"d":"0.30"}]
["28087","Lowndes","MS",{"v":2.0633587211060616,"d":"2.06"},{"v":2.0633587211060616,"d":"2.06"},{"v":0.236282226,"d":"0.24"}]
["28089","Madison","MS",{"v":1.9966004715774393,"d":"2.00"},{"v":1.9966004715774395,"d":"2.00"},{"v":0.201920692,"d":"0.20"}]
["28091","Marion","MS",{"v":2.058023408053837,"d":"2.06"},{"v":2.0580234080538373,"d":"2.06"},{"v":0.306822553,"d":"0.31"}]
["28093","Marshall","MS",{"v":2.111972956258254,"d":"2.11"},{"v":2.1119729562582537,"d":"2.11"},{"v":0.369180843,"d":"0.37"}]
["28095","Monroe","MS",{"v":1.9580888767092555,"d":"1.96"},{"v":1.9580888767092552,"d":"1.96"},{"v":0.287595287,"d":"0.29"}]
["28097","Montgomery","MS",{"v":2.0448952515063037,"d":"2.04"},{"v":2.0448952515063037,"d":"2.04"},{"v":0.290317806,"d":"0.29"}]
["28099","Neshoba","MS",{"v":2.128383232340125,"d":"2.13"},{"v":2.128383232340125,"d":"2.13"},{"v":0.367908184,"d":"0.37"}]
["28101","Newton","MS",{"v":2.0641617505743284,"d":"2.06"},{"v":2.0641617505743284,"d":"2.06"},{"v":0.338245645,"d":"0.34"}]
["28103","Noxubee","MS",{"v":2.241020367476976,"d":"2.24"},{"v":2.241020367476976,"d":"2.24"},{"v":0.292604754,"d":"0.29"}]
["28105","Oktibbeha","MS",{"v":1.9206773643369295,"d":"1.92"},{"v":1.9206773643369293,"d":"1.92"},{"v":0.2874258,"d":"0.29"}]
["28107","Panola","MS",{"v":2.280574907806525,"d":"2.28"},{"v":2.280574907806525,"d":"2.28"},{"v":0.305171487,"d":"0.31"}]
["28109","Pearl River","MS",{"v":1.951441054865845,"d":"1.95"},{"v":1.9514410548658447,"d":"1.95"},{"v":0.279882263,"d":"0.28"}]
["28111","Perry","MS",{"v":2.111727364351933,"d":"2.11"},{"v":2.1117273643519328,"d":"2.11"},{"v":0.38326310199999997,"d":"0.38"}]
["28113","Pike","MS",{"v":1.9717381082882774,"d":"1.97"},{"v":1.9717381082882774,"d":"1.97"},{"v":0.269832585,"d":"0.27"}]
["28115","Pontotoc","MS",{"v":2.15407926939713,"d":"2.15"},{"v":2.15407926939713,"d":"2.15"},{"v":0.325504624,"d":"0.33"}]
["28117","Prentiss","MS",{"v":2.1833342633341783,"d":"2.18"},{"v":2.1833342633341783,"d":"2.18"},{"v":0.327691253,"d":"0.33"}]
["28119","Quitman","MS",{"v":1.8699828479276261,"d":"1.87"},{"v":1.8699828479276261,"d":"1.87"},{"v":0.163779343,"d":"0.16"}]
["28121","Rankin","MS",{"v":2.057926519052573,"d":"2.06"},{"v":2.0579265190525735,"d":"2.06"},{"v":0.255408743,"d":"0.26"}]
["28123","Scott","MS",{"v":2.1651982659883497,"d":"2.17"},{"v":2.1651982659883497,"d":"2.17"},{"v":0.365260758,"d":"0.37"}]
["28125","Sharkey","MS",{"v":2.1380901501063905,"d":"2.14"},{"v":2.1380901501063905,"d":"2.14"},{"v":0.206358452,"d":"0.21"}]
["28127","Simpson","MS",{"v":2.155400824936716,"d":"2.16"},{"v":2.155400824936716,"d":"2.16"},{"v":0.330496943,"d":"0.33"}]
["28129","Smith","MS",{"v":2.109312701172337,"d":"2.11"},{"v":2.109312701172337,"d":"2.11"},{"v":0.372049315,"d":"0.37"}]
["28131","Stone","MS",{"v":2.042297580211688,"d":"2.04"},{"v":2.042297580211688,"d":"2.04"},{"v":0.303258161,"d":"0.30"}]
["28133","Sunflower","MS",{"v":2.146824926753794,"d":"2.15"},{"v":2.1468249267537938,"d":"2.15"},{"v":0.106376969,"d":"0.11"}]
["28135","Tallahatchie","MS",{"v":2.239155560394714,"d":"2.24"},{"v":2.239155560394714,"d":"2.24"},{"v":0.24568844199999998,"d":"0.25"}]
["28137","Tate","MS",{"v":2.4025150515316094,"d":"2.40"},{"v":2.4025150515316094,"d":"2.40"},{"v":0.31456396,"d":"0.31"}]
["28139","Tippah","MS",{"v":2.0051496802920936,"d":"2.01"},{"v":2.0051496802920936,"d":"2.01"},{"v":0.334238051,"d":"0.33"}]
["28141","Tishomingo","MS",{"v":2.166437355173118,"d":"2.17"},{"v":2.166437355173118,"d":"2.17"},{"v":0.413190851,"d":"0.41"}]
["28143","Tunica","MS",{"v":1.6772220240803966,"d":"1.68"},{"v":1.6772220240803966,"d":"1.68"},{"v":0.19528798400000003,"d":"0.20"}]
["28145","Union","MS",{"v":2.1315672729296855,"d":"2.13"},{"v":2.1315672729296855,"d":"2.13"},{"v":0.297995586,"d":"0.30"}]
["28147","Walthall","MS",{"v":1.9652883957113645,"d":"1.97"},{"v":1.9652883957113643,"d":"1.97"},{"v":0.311199125,"d":"0.31"}]
["28149","Warren","MS",{"v":1.917435346189977,"d":"1.92"},{"v":1.9174353461899771,"d":"1.92"},{"v":0.254552839,"d":"0.25"}]
["28151","Washington","MS",{"v":1.6391361244802665,"d":"1.64"},{"v":1.6391361244802665,"d":"1.64"},{"v":0.107449522,"d":"0.11"}]
["28153","Wayne","MS",{"v":2.0615256490073066,"d":"2.06"},{"v":2.061525649007306,"d":"2.06"},{"v":0.334637953,"d":"0.33"}]
["28155","Webster","MS",{"v":2.2242083767242145,"d":"2.22"},{"v":2.2242083767242145,"d":"2.22"},{"v":0.370079999,"d":"0.37"}]
["28157","Wilkinson","MS",{"v":2.018133954182646,"d":"2.02"},{"v":2.018133954182646,"d":"2.02"},{"v":0.384693822,"d":"0.38"}]
["28159","Winston","MS",{"v":2.143768526475327,"d":"2.14"},{"v":2.1437685264753275,"d":"2.14"},{"v":0.367033792,"d":"0.37"}]
["28161","Yalobusha","MS",{"v":2.2627856154178763,"d":"2.26"},{"v":2.2627856154178767,"d":"2.26"},{"v":0.387297102,"d":"0.39"}]
["28163","Yazoo","MS",{"v":2.0550041016262712,"d":"2.06"},{"v":2.0550041016262712,"d":"2.06"},{"v":0.230186226,"d":"0.23"}]
["29001","Adair","MO",{"v":6.809912927934859,"d":"6.81"},{"v":6.80991292793486,"d":"6.81"},{"v":0.885769795,"d":"0.89"}]
["29003","Andrew","MO",{"v":6.4134505707375045,"d":"6.41"},{"v":6.4134505707375045,"d":"6.41"},{"v":1.00509897,"d":"1.01"}]
["29005","Atchison","MO",{"v":6.215003456386912,"d":"6.22"},{"v":6.2150034563869125,"d":"6.22"},{"v":0.918284407,"d":"0.92"}]
["29007","Audrain","MO",{"v":6.413179625163166,"d":"6.41"},{"v":6.413179625163166,"d":"6.41"},{"v":0.729130615,"d":"0.73"}]
["29009","Barry","MO",{"v":6.9113310159741115,"d":"6.91"},{"v":6.911331015974112,"d":"6.91"},{"v":1.102115569,"d":"1.10"}]
["29011","Barton","MO",{"v":6.152027276400806,"d":"6.15"},{"v":6.152027276400806,"d":"6.15"},{"v":0.668959879,"d":"0.67"}]
["29013","Bates","MO",{"v":6.351821789805971,"d":"6.35"},{"v":6.351821789805972,"d":"6.35"},{"v":0.805030436,"d":"0.81"}]
["29015","Benton","MO",{"v":7.150729175103419,"d":"7.15"},{"v":7.15072917510342,"d":"7.15"},{"v":1.303506879,"d":"1.30"}]
["29017","Bollinger","MO",{"v":7.333119349573272,"d":"7.33"},{"v":7.3331193495732725,"d":"7.33"},{"v":1.442874855,"d":"1.44"}]
["29019","Boone","MO",{"v":6.280544911157769,"d":"6.28"},{"v":6.280544911157769,"d":"6.28"},{"v":0.876099739,"d":"0.88"}]
["29021","Buchanan","MO",{"v":5.995107093421872,"d":"6.00"},{"v":5.995107093421872,"d":"6.00"},{"v":0.742703409,"d":"0.74"}]
["29023","Butler","MO",{"v":6.409471353222794,"d":"6.41"},{"v":6.409471353222793,"d":"6.41"},{"v":0.812755834,"d":"0.81"}]
["29025","Caldwell","MO",{"v":6.541795433222389,"d":"6.54"},{"v":6.541795433222389,"d":"6.54"},{"v":1.261223192,"d":"1.26"}]
["29027","Callaway","MO",{"v":6.871637958669175,"d":"6.87"},{"v":6.871637958669174,"d":"6.87"},{"v":1.271986196,"d":"1.27"}]
["29029","Camden","MO",{"v":7.218895213790805,"d":"7.22"},{"v":7.218895213790805,"d":"7.22"},{"v":1.555690624,"d":"1.56"}]
["29031","Cape Girardeau","MO",{"v":6.417445678916996,"d":"6.42"},{"v":6.417445678916998,"d":"6.42"},{"v":0.731118266,"d":"0.73"}]
["29033","Carroll","MO",{"v":5.950162719574778,"d":"5.95"},{"v":5.950162719574778,"d":"5.95"},{"v":0.906184206,"d":"0.91"}]
["29035","Carter","MO",{"v":7.632951009811697,"d":"7.63"},{"v":7.632951009811697,"d":"7.63"},{"v":2.215618886,"d":"2.22"}]
["29037","Cass","MO",{"v":5.595560896074682,"d":"5.60"},{"v":5.595560896074683,"d":"5.60"},{"v":0.616751735,"d":"0.62"}]
["29039","Cedar","MO",{"v":6.918916824557567,"d":"6.92"},{"v":6.918916824557568,"d":"6.92"},{"v":1.055310001,"d":"1.06"}]
["29041","Chariton","MO",{"v":7.075498541062556,"d":"7.08"},{"v":7.075498541062555,"d":"7.08"},{"v":1.135780425,"d":"1.14"}]
["29043","Christian","MO",{"v":6.557431843449318,"d":"6.56"},{"v":6.557431843449318,"d":"6.56"},{"v":0.930775714,"d":"0.93"}]
["29045","Clark","MO",{"v":7.194072943512931,"d":"7.19"},{"v":7.194072943512931,"d":"7.19"},{"v":1.12832216,"d":"1.13"}]
["29047","Clay","MO",{"v":5.829985115504623,"d":"5.83"},{"v":5.829985115504623,"d":"5.83"},{"v":0.809808291,"d":"0.81"}]
["29049","Clinton","MO",{"v":6.37667001125037,"d":"6.38"},{"v":6.37667001125037,"d":"6.38"},{"v":0.936849899,"d":"0.94"}]
["29051","Cole","MO",{"v":6.465412973542991,"d":"6.47"},{"v":6.465412973542992,"d":"6.47"},{"v":0.883641239,"d":"0.88"}]
["29053","Cooper","MO",{"v":6.704484138437544,"d":"6.70"},{"v":6.704484138437544,"d":"6.70"},{"v":0.780462682,"d":"0.78"}]
["29055","Crawford","MO",{"v":7.017775490246047,"d":"7.02"},{"v":7.017775490246047,"d":"7.02"},{"v":1.407555651,"d":"1.41"}]
["29057","Dade","MO",{"v":6.805324361154228,"d":"6.81"},{"v":6.805324361154229,"d":"6.81"},{"v":0.8754351680000001,"d":"0.88"}]
["29059","Dallas","MO",{"v":7.133628199418776,"d":"7.13"},{"v":7.133628199418776,"d":"7.13"},{"v":1.242470834,"d":"1.24"}]
["29061","Daviess","MO",{"v":6.718376494853753,"d":"6.72"},{"v":6.718376494853753,"d":"6.72"},{"v":1.139620309,"d":"1.14"}]
["29063","Dekalb","MO",{"v":6.808218224385069,"d":"6.81"},{"v":6.808218224385069,"d":"6.81"},{"v":1.109649634,"d":"1.11"}]
["29065","Dent","MO",{"v":7.264965989276355,"d":"7.26"},{"v":7.264965989276354,"d":"7.26"},{"v":1.418919755,"d":"1.42"}]
["29067","Douglas","MO",{"v":7.107421634476913,"d":"7.11"},{"v":7.107421634476912,"d":"7.11"},{"v":1.326507952,"d":"1.33"}]
["29069","Dunklin","MO",{"v":5.570614955980103,"d":"5.57"},{"v":5.570614955980102,"d":"5.57"},{"v":0.464667964,"d":"0.46"}]
["29071","Franklin","MO",{"v":7.096149283545101,"d":"7.10"},{"v":7.0961492835451,"d":"7.10"},{"v":1.4967997949999998,"d":"1.50"}]
["29073","Gasconade","MO",{"v":7.13377209096461,"d":"7.13"},{"v":7.13377209096461,"d":"7.13"},{"v":1.577266698,"d":"1.58"}]
["29075","Gentry","MO",{"v":6.587268954290957,"d":"6.59"},{"v":6.587268954290957,"d":"6.59"},{"v":1.023087167,"d":"1.02"}]
["29077","Greene","MO",{"v":6.063924933328424,"d":"6.06"},{"v":6.063924933328424,"d":"6.06"},{"v":0.636240689,"d":"0.64"}]
["29079","Grundy","MO",{"v":6.947441379558288,"d":"6.95"},{"v":6.9474413795582874,"d":"6.95"},{"v":0.907539549,"d":"0.91"}]
["29081","Harrison","MO",{"v":6.778133951862704,"d":"6.78"},{"v":6.778133951862702,"d":"6.78"},{"v":0.992908551,"d":"0.99"}]
["29083","Henry","MO",{"v":6.417840285846219,"d":"6.42"},{"v":6.41784028584622,"d":"6.42"},{"v":0.785132197,"d":"0.79"}]
["29085","Hickory","MO",{"v":7.547799320743222,"d":"7.55"},{"v":7.54779932074322,"d":"7.55"},{"v":1.520714769,"d":"1.52"}]
["29087","Holt","MO",{"v":5.091633276636371,"d":"5.09"},{"v":5.0916332766363706,"d":"5.09"},{"v":1.013532427,"d":"1.01"}]
["29089","Howard","MO",{"v":7.187905007751661,"d":"7.19"},{"v":7.18790500775166,"d":"7.19"},{"v":1.089150329,"d":"1.09"}]
["29091","Howell","MO",{"v":7.024164355324395,"d":"7.02"},{"v":7.024164355324394,"d":"7.02"},{"v":1.220190085,"d":"1.22"}]
["29093","Iron","MO",{"v":6.774142789217547,"d":"6.77"},{"v":6.774142789217547,"d":"6.77"},{"v":1.674173365,"d":"1.67"}]
["29095","Jackson","MO",{"v":3.4645327378955857,"d":"3.46"},{"v":3.464532737895585,"d":"3.46"},{"v":1.067155528,"d":"1.07"}]
["29097","Jasper","MO",{"v":6.144564960894687,"d":"6.14"},{"v":6.144564960894687,"d":"6.14"},{"v":0.599454028,"d":"0.60"}]
["29099","Jefferson","MO",{"v":6.673831807417528,"d":"6.67"},{"v":6.673831807417527,"d":"6.67"},{"v":1.224383877,"d":"1.22"}]
["29101","Johnson","MO",{"v":6.32424631543959,"d":"6.32"},{"v":6.3242463154395905,"d":"6.32"},{"v":0.800721977,"d":"0.80"}]
["29103","Knox","MO",{"v":7.067050565451848,"d":"7.07"},{"v":7.067050565451847,"d":"7.07"},{"v":1.031257864,"d":"1.03"}]
["29105","Laclede","MO",{"v":6.969340518633366,"d":"6.97"},{"v":6.9693405186333655,"d":"6.97"},{"v":1.165847363,"d":"1.17"}]
["29107","Lafayette","MO",{"v":6.16237406551579,"d":"6.16"},{"v":6.162374065515791,"d":"6.16"},{"v":0.879009565,"d":"0.88"}]
["29109","Lawrence","MO",{"v":6.479532123131417,"d":"6.48"},{"v":6.479532123131418,"d":"6.48"},{"v":0.720341057,"d":"0.72"}]
["29111","Lewis","MO",{"v":6.835813712297135,"d":"6.84"},{"v":6.835813712297136,"d":"6.84"},{"v":1.023709889,"d":"1.02"}]
["29113","Lincoln","MO",{"v":7.1048595165768145,"d":"7.10"},{"v":7.104859516576814,"d":"7.10"},{"v":1.299401739,"d":"1.30"}]
["29115","Linn","MO",{"v":6.665683509463734,"d":"6.67"},{"v":6.665683509463733,"d":"6.67"},{"v":0.936566413,"d":"0.94"}]
["29117","Livingston","MO",{"v":6.742870561655941,"d":"6.74"},{"v":6.742870561655941,"d":"6.74"},{"v":0.8415067560000001,"d":"0.84"}]
["29119","Mcdonald","MO",{"v":7.110137022391393,"d":"7.11"},{"v":7.110137022391393,"d":"7.11"},{"v":1.401241565,"d":"1.40"}]
["29121","Macon","MO",{"v":7.033079080461839,"d":"7.03"},{"v":7.033079080461839,"d":"7.03"},{"v":1.007436793,"d":"1.01"}]
["29123","Madison","MO",{"v":7.252560992761314,"d":"7.25"},{"v":7.252560992761314,"d":"7.25"},{"v":1.4779224819999999,"d":"1.48"}]
["29125","Maries","MO",{"v":7.078479494308375,"d":"7.08"},{"v":7.078479494308375,"d":"7.08"},{"v":1.396204331,"d":"1.40"}]
["29127","Marion","MO",{"v":6.324455166254053,"d":"6.32"},{"v":6.324455166254053,"d":"6.32"},{"v":0.696547101,"d":"0.70"}]
["29129","Mercer","MO",{"v":6.177345984766951,"d":"6.18"},{"v":6.1773459847669505,"d":"6.18"},{"v":1.173754183,"d":"1.17"}]
["29131","Miller","MO",{"v":7.083791080936545,"d":"7.08"},{"v":7.083791080936545,"d":"7.08"},{"v":1.379299482,"d":"1.38"}]
["29133","Mississippi","MO",{"v":6.061712932040946,"d":"6.06"},{"v":6.061712932040946,"d":"6.06"},{"v":0.465117027,"d":"0.47"}]
["29135","Moniteau","MO",{"v":6.1054003550083085,"d":"6.11"},{"v":6.1054003550083085,"d":"6.11"},{"v":0.782668857,"d":"0.78"}]
["29137","Monroe","MO",{"v":7.142866122333886,"d":"7.14"},{"v":7.142866122333887,"d":"7.14"},{"v":1.00371619,"d":"1.00"}]
["29139","Montgomery","MO",{"v":7.037909362501281,"d":"7.04"},{"v":7.0379093625012805,"d":"7.04"},{"v":1.191240903,"d":"1.19"}]
["29141","Morgan","MO",{"v":7.067068727337907,"d":"7.07"},{"v":7.067068727337907,"d":"7.07"},{"v":1.411992394,"d":"1.41"}]
["29143","New Madrid","MO",{"v":5.980862752583891,"d":"5.98"},{"v":5.980862752583891,"d":"5.98"},{"v":0.515038017,"d":"0.52"}]
["29145","Newton","MO",{"v":6.780950127392082,"d":"6.78"},{"v":6.7809501273920825,"d":"6.78"},{"v":0.908401598,"d":"0.91"}]
["29147","Nodaway","MO",{"v":6.3788880954554585,"d":"6.38"},{"v":6.378888095455458,"d":"6.38"},{"v":0.878767902,"d":"0.88"}]
["29149","Oregon","MO",{"v":7.423729639122326,"d":"7.42"},{"v":7.423729639122326,"d":"7.42"},{"v":1.570226369,"d":"1.57"}]
["29151","Osage","MO",{"v":7.2679784786205595,"d":"7.27"},{"v":7.267978478620561,"d":"7.27"},{"v":1.655538217,"d":"1.66"}]
["29153","Ozark","MO",{"v":7.387984064303865,"d":"7.39"},{"v":7.387984064303866,"d":"7.39"},{"v":1.534924017,"d":"1.53"}]
["29155","Pemiscot","MO",{"v":5.1559172925465555,"d":"5.16"},{"v":5.1559172925465555,"d":"5.16"},{"v":0.468127985,"d":"0.47"}]
["29157","Perry","MO",{"v":6.678290628433009,"d":"6.68"},{"v":6.6782906284330075,"d":"6.68"},{"v":0.9218768729999999,"d":"0.92"}]
["29159","Pettis","MO",{"v":6.324959956866247,"d":"6.32"},{"v":6.324959956866247,"d":"6.32"},{"v":0.649585152,"d":"0.65"}]
["29161","Phelps","MO",{"v":6.653353715964018,"d":"6.65"},{"v":6.653353715964017,"d":"6.65"},{"v":1.306598765,"d":"1.31"}]
["29163","Pike","MO",{"v":7.106763777046932,"d":"7.11"},{"v":7.1067637770469325,"d":"7.11"},{"v":1.038383576,"d":"1.04"}]
["29165","Platte","MO",{"v":5.948287646544499,"d":"5.95"},{"v":5.948287646544499,"d":"5.95"},{"v":0.77084543,"d":"0.77"}]
["29167","Polk","MO",{"v":6.957151607030646,"d":"6.96"},{"v":6.957151607030647,"d":"6.96"},{"v":1.044773905,"d":"1.04"}]
["29169","Pulaski","MO",{"v":7.013765085424438,"d":"7.01"},{"v":7.0137650854244376,"d":"7.01"},{"v":1.473474595,"d":"1.47"}]
["29171","Putnam","MO",{"v":7.511181432436946,"d":"7.51"},{"v":7.511181432436946,"d":"7.51"},{"v":1.170365264,"d":"1.17"}]
["29173","Ralls","MO",{"v":6.682630389162821,"d":"6.68"},{"v":6.682630389162821,"d":"6.68"},{"v":1.153854633,"d":"1.15"}]
["29175","Randolph","MO",{"v":6.601906557022533,"d":"6.60"},{"v":6.601906557022532,"d":"6.60"},{"v":0.8975223829999999,"d":"0.90"}]
["29177","Ray","MO",{"v":6.255232145540958,"d":"6.26"},{"v":6.255232145540958,"d":"6.26"},{"v":1.060548042,"d":"1.06"}]
["29179","Reynolds","MO",{"v":7.545876588678112,"d":"7.55"},{"v":7.5458765886781105,"d":"7.55"},{"v":2.037086712,"d":"2.04"}]
["29181","Ripley","MO",{"v":7.356222758952271,"d":"7.36"},{"v":7.356222758952271,"d":"7.36"},{"v":1.656338988,"d":"1.66"}]
["29183","St Charles","MO",{"v":6.006660953223901,"d":"6.01"},{"v":6.006660953223901,"d":"6.01"},{"v":0.8570613730000001,"d":"0.86"}]
["29185","St Clair","MO",{"v":6.66370102287076,"d":"6.66"},{"v":6.663701022870761,"d":"6.66"},{"v":1.32854102,"d":"1.33"}]
["29186","Ste Genevieve","MO",{"v":6.912239215008889,"d":"6.91"},{"v":6.912239215008889,"d":"6.91"},{"v":1.292139849,"d":"1.29"}]
["29187","St Francois","MO",{"v":6.934819985818802,"d":"6.93"},{"v":6.934819985818801,"d":"6.93"},{"v":1.189045844,"d":"1.19"}]
["29189","St Louis","MO",{"v":0.31591880582010445,"d":"0.32"},{"v":0.31591880582010456,"d":"0.32"},{"v":1.716469854,"d":"1.72"}]
["29195","Saline","MO",{"v":6.641800371629313,"d":"6.64"},{"v":6.641800371629313,"d":"6.64"},{"v":0.783440143,"d":"0.78"}]
["29197","Schuyler","MO",{"v":6.8750950450488215,"d":"6.88"},{"v":6.8750950450488215,"d":"6.88"},{"v":1.072899273,"d":"1.07"}]
["29199","Scotland","MO",{"v":6.680610268153469,"d":"6.68"},{"v":6.680610268153469,"d":"6.68"},{"v":0.989027288,"d":"0.99"}]
["29201","Scott","MO",{"v":6.068659045244098,"d":"6.07"},{"v":6.068659045244097,"d":"6.07"},{"v":0.542307671,"d":"0.54"}]
["29203","Shannon","MO",{"v":7.532459091894729,"d":"7.53"},{"v":7.532459091894729,"d":"7.53"},{"v":2.01208206,"d":"2.01"}]
["29205","Shelby","MO",{"v":7.1653231820833305,"d":"7.17"},{"v":7.1653231820833305,"d":"7.17"},{"v":1.06028771,"d":"1.06"}]
["29207","Stoddard","MO",{"v":6.3966549103298895,"d":"6.40"},{"v":6.39665491032989,"d":"6.40"},{"v":0.605488216,"d":"0.61"}]
["29209","Stone","MO",{"v":7.198710980130297,"d":"7.20"},{"v":7.198710980130297,"d":"7.20"},{"v":1.377301331,"d":"1.38"}]
["29211","Sullivan","MO",{"v":7.205416726090344,"d":"7.21"},{"v":7.205416726090345,"d":"7.21"},{"v":1.172602059,"d":"1.17"}]
["29213","Taney","MO",{"v":7.1068819459908426,"d":"7.11"},{"v":7.106881945990843,"d":"7.11"},{"v":1.399839879,"d":"1.40"}]
["29215","Texas","MO",{"v":7.4010814848337425,"d":"7.40"},{"v":7.401081484833741,"d":"7.40"},{"v":1.543433206,"d":"1.54"}]
["29217","Vernon","MO",{"v":6.696538753486066,"d":"6.70"},{"v":6.696538753486067,"d":"6.70"},{"v":0.81986372,"d":"0.82"}]
["29219","Warren","MO",{"v":7.298931412803662,"d":"7.30"},{"v":7.298931412803662,"d":"7.30"},{"v":1.507287371,"d":"1.51"}]
["29221","Washington","MO",{"v":7.445176094109193,"d":"7.45"},{"v":7.445176094109194,"d":"7.45"},{"v":1.7704406929999998,"d":"1.77"}]
["29223","Wayne","MO",{"v":7.432478688188384,"d":"7.43"},{"v":7.432478688188383,"d":"7.43"},{"v":1.918044469,"d":"1.92"}]
["29225","Webster","MO",{"v":7.017198607796867,"d":"7.02"},{"v":7.017198607796866,"d":"7.02"},{"v":1.056565308,"d":"1.06"}]
["29227","Worth","MO",{"v":6.175109917864115,"d":"6.18"},{"v":6.1751099178641145,"d":"6.18"},{"v":1.099588886,"d":"1.10"}]
["29229","Wright","MO",{"v":6.952333139649542,"d":"6.95"},{"v":6.952333139649542,"d":"6.95"},{"v":1.101382831,"d":"1.10"}]
["29510","St Louis City","MO",{"v":1.1908326352073436E-7,"d":"0.00"},{"v":1.1908326352073432E-7,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["30001","Beaverhead","MT",{"v":2.061063927546404,"d":"2.06"},{"v":2.0610639275464044,"d":"2.06"},{"v":0.886804026,"d":"0.89"}]
["30003","Big Horn","MT",{"v":2.015467816828595,"d":"2.02"},{"v":2.0154678168285955,"d":"2.02"},{"v":0.648696826,"d":"0.65"}]
["30005","Blaine","MT",{"v":2.0616684458025465,"d":"2.06"},{"v":2.0616684458025465,"d":"2.06"},{"v":0.779951156,"d":"0.78"}]
["30007","Broadwater","MT",{"v":2.061383355497797,"d":"2.06"},{"v":2.0613833554977976,"d":"2.06"},{"v":0.956086791,"d":"0.96"}]
["30009","Carbon","MT",{"v":1.9675996513562464,"d":"1.97"},{"v":1.9675996513562464,"d":"1.97"},{"v":0.6276920660000002,"d":"0.63"}]
["30011","Carter","MT",{"v":2.0383169980288462,"d":"2.04"},{"v":2.038316998028846,"d":"2.04"},{"v":0.856897357,"d":"0.86"}]
["30013","Cascade","MT",{"v":1.9204588995789365,"d":"1.92"},{"v":1.9204588995789362,"d":"1.92"},{"v":0.422051169,"d":"0.42"}]
["30015","Chouteau","MT",{"v":2.048927944983022,"d":"2.05"},{"v":2.048927944983022,"d":"2.05"},{"v":0.793848785,"d":"0.79"}]
["30017","Custer","MT",{"v":1.9553712773412213,"d":"1.96"},{"v":1.9553712773412213,"d":"1.96"},{"v":0.410697962,"d":"0.41"}]
["30019","Daniels","MT",{"v":2.1100391464368404,"d":"2.11"},{"v":2.1100391464368404,"d":"2.11"},{"v":1.033808009,"d":"1.03"}]
["30021","Dawson","MT",{"v":1.9979705474902225,"d":"2.00"},{"v":1.9979705474902227,"d":"2.00"},{"v":0.53559762,"d":"0.54"}]
["30023","Deer Lodge","MT",{"v":1.9821469344697284,"d":"1.98"},{"v":1.9821469344697282,"d":"1.98"},{"v":0.62708996,"d":"0.63"}]
["30025","Fallon","MT",{"v":2.0184580484474184,"d":"2.02"},{"v":2.0184580484474184,"d":"2.02"},{"v":0.632519873,"d":"0.63"}]
["30027","Fergus","MT",{"v":1.985262043547221,"d":"1.99"},{"v":1.9852620435472208,"d":"1.99"},{"v":0.551382406,"d":"0.55"}]
["30029","Flathead","MT",{"v":2.0410880191815486,"d":"2.04"},{"v":2.0410880191815486,"d":"2.04"},{"v":1.010387877,"d":"1.01"}]
["30031","Gallatin","MT",{"v":2.0314671542279643,"d":"2.03"},{"v":2.0314671542279643,"d":"2.03"},{"v":0.768540597,"d":"0.77"}]
["30033","Garfield","MT",{"v":2.1093764375603925,"d":"2.11"},{"v":2.109376437560392,"d":"2.11"},{"v":1.057704719,"d":"1.06"}]
["30035","Glacier","MT",{"v":2.035210388448146,"d":"2.04"},{"v":2.035210388448146,"d":"2.04"},{"v":0.748911362,"d":"0.75"}]
["30037","Golden Valley","MT",{"v":2.048260403435042,"d":"2.05"},{"v":2.0482604034350422,"d":"2.05"},{"v":0.916001806,"d":"0.92"}]
["30039","Granite","MT",{"v":2.1008030479870596,"d":"2.10"},{"v":2.100803047987059,"d":"2.10"},{"v":1.096546211,"d":"1.10"}]
["30041","Hill","MT",{"v":1.9953748211989755,"d":"2.00"},{"v":1.9953748211989755,"d":"2.00"},{"v":0.529591776,"d":"0.53"}]
["30043","Jefferson","MT",{"v":2.046222254146116,"d":"2.05"},{"v":2.0462222541461155,"d":"2.05"},{"v":1.042593814,"d":"1.04"}]
["30045","Judith Basin","MT",{"v":2.066521228688962,"d":"2.07"},{"v":2.066521228688962,"d":"2.07"},{"v":1.0053866,"d":"1.01"}]
["30047","Lake","MT",{"v":2.093702861588828,"d":"2.09"},{"v":2.093702861588828,"d":"2.09"},{"v":1.199981529,"d":"1.20"}]
["30049","Lewis and Clark","MT",{"v":1.9633932261903353,"d":"1.96"},{"v":1.9633932261903353,"d":"1.96"},{"v":0.608047566,"d":"0.61"}]
["30051","Liberty","MT",{"v":2.03519533040565,"d":"2.04"},{"v":2.03519533040565,"d":"2.04"},{"v":0.680686125,"d":"0.68"}]
["30053","Lincoln","MT",{"v":2.169148727872443,"d":"2.17"},{"v":2.1691487278724435,"d":"2.17"},{"v":1.731715416,"d":"1.73"}]
["30055","McCone","MT",{"v":2.103323877206066,"d":"2.10"},{"v":2.103323877206066,"d":"2.10"},{"v":1.031158734,"d":"1.03"}]
["30057","Madison","MT",{"v":2.105908113318345,"d":"2.11"},{"v":2.1059081133183453,"d":"2.11"},{"v":1.174276469,"d":"1.17"}]
["30059","Meagher","MT",{"v":2.037690292775822,"d":"2.04"},{"v":2.037690292775822,"d":"2.04"},{"v":1.119308282,"d":"1.12"}]
["30061","Mineral","MT",{"v":2.195952289045093,"d":"2.20"},{"v":2.195952289045093,"d":"2.20"},{"v":1.6789548310000002,"d":"1.68"}]
["30063","Missoula","MT",{"v":1.9796332057781538,"d":"1.98"},{"v":1.9796332057781538,"d":"1.98"},{"v":0.731518349,"d":"0.73"}]
["30065","Musselshell","MT",{"v":2.0596447594926315,"d":"2.06"},{"v":2.0596447594926315,"d":"2.06"},{"v":0.918125314,"d":"0.92"}]
["30067","Park","MT",{"v":1.9994969235148008,"d":"2.00"},{"v":1.9994969235148008,"d":"2.00"},{"v":0.723012549,"d":"0.72"}]
["30069","Petroleum","MT",{"v":2.0668745245079796,"d":"2.07"},{"v":2.0668745245079796,"d":"2.07"},{"v":0.90410711,"d":"0.90"}]
["30071","Phillips","MT",{"v":2.0413344790086017,"d":"2.04"},{"v":2.0413344790086017,"d":"2.04"},{"v":0.706678667,"d":"0.71"}]
["30073","Pondera","MT",{"v":2.0183912201531555,"d":"2.02"},{"v":2.0183912201531555,"d":"2.02"},{"v":0.641147129,"d":"0.64"}]
["30075","Powder River","MT",{"v":2.056779992388625,"d":"2.06"},{"v":2.0567799923886256,"d":"2.06"},{"v":0.92801957,"d":"0.93"}]
["30077","Powell","MT",{"v":2.0194011325415224,"d":"2.02"},{"v":2.019401132541522,"d":"2.02"},{"v":0.7716482269999999,"d":"0.77"}]
["30079","Prairie","MT",{"v":2.028421980205542,"d":"2.03"},{"v":2.0284219802055423,"d":"2.03"},{"v":0.668548265,"d":"0.67"}]
["30081","Ravalli","MT",{"v":2.041083883286335,"d":"2.04"},{"v":2.0410838832863347,"d":"2.04"},{"v":0.914552626,"d":"0.91"}]
["30083","Richland","MT",{"v":2.0600527477544417,"d":"2.06"},{"v":2.0600527477544417,"d":"2.06"},{"v":0.621950943,"d":"0.62"}]
["30085","Roosevelt","MT",{"v":2.045687233039734,"d":"2.05"},{"v":2.0456872330397347,"d":"2.05"},{"v":0.646229162,"d":"0.65"}]
["30087","Rosebud","MT",{"v":2.0222439218547166,"d":"2.02"},{"v":2.0222439218547166,"d":"2.02"},{"v":0.78813614,"d":"0.79"}]
["30089","Sanders","MT",{"v":2.149870546832634,"d":"2.15"},{"v":2.149870546832634,"d":"2.15"},{"v":1.497300585,"d":"1.50"}]
["30091","Sheridan","MT",{"v":2.1046871132970786,"d":"2.10"},{"v":2.1046871132970786,"d":"2.10"},{"v":1.042613358,"d":"1.04"}]
["30093","Silver Bow","MT",{"v":1.9784146624815848,"d":"1.98"},{"v":1.9784146624815846,"d":"1.98"},{"v":0.591491263,"d":"0.59"}]
["30095","Stillwater","MT",{"v":1.9846095598416797,"d":"1.98"},{"v":1.9846095598416797,"d":"1.98"},{"v":0.655137782,"d":"0.66"}]
["30097","Sweet Grass","MT",{"v":1.9900562927400234,"d":"1.99"},{"v":1.9900562927400234,"d":"1.99"},{"v":0.71073395,"d":"0.71"}]
["30099","Teton","MT",{"v":2.052233802318973,"d":"2.05"},{"v":2.052233802318973,"d":"2.05"},{"v":0.82600641,"d":"0.83"}]
["30101","Toole","MT",{"v":2.0374098724150222,"d":"2.04"},{"v":2.0374098724150222,"d":"2.04"},{"v":0.607204713,"d":"0.61"}]
["30103","Treasure","MT",{"v":2.065585460126443,"d":"2.07"},{"v":2.065585460126443,"d":"2.07"},{"v":0.861295068,"d":"0.86"}]
["30105","Valley","MT",{"v":2.0163872309237934,"d":"2.02"},{"v":2.0163872309237934,"d":"2.02"},{"v":0.63235889,"d":"0.63"}]
["30107","Wheatland","MT",{"v":1.9918237766627265,"d":"1.99"},{"v":1.9918237766627263,"d":"1.99"},{"v":0.669270603,"d":"0.67"}]
["30109","Wibaux","MT",{"v":2.0037970435658776,"d":"2.00"},{"v":2.0037970435658776,"d":"2.00"},{"v":0.675875102,"d":"0.68"}]
["30111","Yellowstone","MT",{"v":1.9061302126229187,"d":"1.91"},{"v":1.9061302126229185,"d":"1.91"},{"v":0.38117,"d":"0.38"}]
["31001","Adams","NE",{"v":1.863434298592025,"d":"1.86"},{"v":1.8634342985920245,"d":"1.86"},{"v":0.216277461,"d":"0.22"}]
["31003","Antelope","NE",{"v":1.9939501401845696,"d":"1.99"},{"v":1.9939501401845696,"d":"1.99"},{"v":0.44245111499999995,"d":"0.44"}]
["31005","Arthur","NE",{"v":2.231969891605651,"d":"2.23"},{"v":2.231969891605651,"d":"2.23"},{"v":0.54118795,"d":"0.54"}]
["31007","Banner","NE",{"v":2.105342289515022,"d":"2.11"},{"v":2.105342289515022,"d":"2.11"},{"v":0.503448204,"d":"0.50"}]
["31009","Blaine","NE",{"v":2.309228834571018,"d":"2.31"},{"v":2.309228834571018,"d":"2.31"},{"v":0.5318153880000001,"d":"0.53"}]
["31011","Boone","NE",{"v":2.067643309786886,"d":"2.07"},{"v":2.0676433097868863,"d":"2.07"},{"v":0.453770254,"d":"0.45"}]
["31013","Box Butte","NE",{"v":1.766769998568485,"d":"1.77"},{"v":1.766769998568485,"d":"1.77"},{"v":0.266198308,"d":"0.27"}]
["31015","Boyd","NE",{"v":2.2003480186637097,"d":"2.20"},{"v":2.2003480186637097,"d":"2.20"},{"v":0.558959096,"d":"0.56"}]
["31017","Brown","NE",{"v":2.0379900751458564,"d":"2.04"},{"v":2.0379900751458564,"d":"2.04"},{"v":0.422552723,"d":"0.42"}]
["31019","Buffalo","NE",{"v":2.037077089752124,"d":"2.04"},{"v":2.0370770897521244,"d":"2.04"},{"v":0.282105562,"d":"0.28"}]
["31021","Burt","NE",{"v":2.0707066107184535,"d":"2.07"},{"v":2.0707066107184535,"d":"2.07"},{"v":0.43628944,"d":"0.44"}]
["31023","Butler","NE",{"v":1.554040914516675,"d":"1.55"},{"v":1.5540409145166751,"d":"1.55"},{"v":0.376417902,"d":"0.38"}]
["31025","Cass","NE",{"v":2.0143344257029616,"d":"2.01"},{"v":2.0143344257029616,"d":"2.01"},{"v":0.363084468,"d":"0.36"}]
["31027","Cedar","NE",{"v":2.0201896450319197,"d":"2.02"},{"v":2.0201896450319192,"d":"2.02"},{"v":0.4435977300000001,"d":"0.44"}]
["31029","Chase","NE",{"v":2.0031012033202047,"d":"2.00"},{"v":2.003101203320205,"d":"2.00"},{"v":0.333169301,"d":"0.33"}]
["31031","Cherry","NE",{"v":2.0603914587886387,"d":"2.06"},{"v":2.0603914587886387,"d":"2.06"},{"v":0.454742563,"d":"0.45"}]
["31033","Cheyenne","NE",{"v":1.950844459047198,"d":"1.95"},{"v":1.950844459047198,"d":"1.95"},{"v":0.26786983,"d":"0.27"}]
["31035","Clay","NE",{"v":1.8181280077036137,"d":"1.82"},{"v":1.8181280077036135,"d":"1.82"},{"v":0.304707942,"d":"0.30"}]
["31037","Colfax","NE",{"v":1.9810586152393854,"d":"1.98"},{"v":1.9810586152393852,"d":"1.98"},{"v":0.356490258,"d":"0.36"}]
["31039","Cuming","NE",{"v":2.158686180556809,"d":"2.16"},{"v":2.158686180556809,"d":"2.16"},{"v":0.397326044,"d":"0.40"}]
["31041","Custer","NE",{"v":2.1794526530624756,"d":"2.18"},{"v":2.179452653062475,"d":"2.18"},{"v":0.371600533,"d":"0.37"}]
["31043","Dakota","NE",{"v":1.9818686625593211,"d":"1.98"},{"v":1.9818686625593211,"d":"1.98"},{"v":0.343885713,"d":"0.34"}]
["31045","Dawes","NE",{"v":2.053444503570733,"d":"2.05"},{"v":2.053444503570733,"d":"2.05"},{"v":0.31917279,"d":"0.32"}]
["31047","Dawson","NE",{"v":2.0363058254439856,"d":"2.04"},{"v":2.0363058254439856,"d":"2.04"},{"v":0.29696741,"d":"0.30"}]
["31049","Deuel","NE",{"v":2.0742031058744512,"d":"2.07"},{"v":2.074203105874451,"d":"2.07"},{"v":0.321774758,"d":"0.32"}]
["31051","Dixon","NE",{"v":2.083464184108988,"d":"2.08"},{"v":2.0834641841089883,"d":"2.08"},{"v":0.473046743,"d":"0.47"}]
["31053","Dodge","NE",{"v":1.8432786461468613,"d":"1.84"},{"v":1.8432786461468613,"d":"1.84"},{"v":0.262093653,"d":"0.26"}]
["31055","Douglas","NE",{"v":0.33615489027019213,"d":"0.34"},{"v":0.33615489027019213,"d":"0.34"},{"v":0.511587577,"d":"0.51"}]
["31057","Dundy","NE",{"v":2.079367693470771,"d":"2.08"},{"v":2.079367693470771,"d":"2.08"},{"v":0.338937592,"d":"0.34"}]
["31059","Fillmore","NE",{"v":2.0483495891907766,"d":"2.05"},{"v":2.0483495891907766,"d":"2.05"},{"v":0.308325258,"d":"0.31"}]
["31061","Franklin","NE",{"v":1.823717098429706,"d":"1.82"},{"v":1.8237170984297058,"d":"1.82"},{"v":0.297864178,"d":"0.30"}]
["31063","Frontier","NE",{"v":2.0117746290506653,"d":"2.01"},{"v":2.0117746290506653,"d":"2.01"},{"v":0.35478186100000003,"d":"0.35"}]
["31065","Furnas","NE",{"v":2.0459227395894457,"d":"2.05"},{"v":2.0459227395894457,"d":"2.05"},{"v":0.299124742,"d":"0.30"}]
["31067","Gage","NE",{"v":2.18818284302085,"d":"2.19"},{"v":2.18818284302085,"d":"2.19"},{"v":0.272315865,"d":"0.27"}]
["31069","Garden","NE",{"v":2.1478602746208093,"d":"2.15"},{"v":2.147860274620809,"d":"2.15"},{"v":0.39410125099999993,"d":"0.39"}]
["31071","Garfield","NE",{"v":2.0568015636773995,"d":"2.06"},{"v":2.0568015636773995,"d":"2.06"},{"v":0.412652118,"d":"0.41"}]
["31073","Gosper","NE",{"v":2.0926716569212935,"d":"2.09"},{"v":2.0926716569212935,"d":"2.09"},{"v":0.342320034,"d":"0.34"}]
["31075","Grant","NE",{"v":2.239406919980582,"d":"2.24"},{"v":2.2394069199805826,"d":"2.24"},{"v":0.541424081,"d":"0.54"}]
["31077","Greeley","NE",{"v":2.148048568232355,"d":"2.15"},{"v":2.148048568232355,"d":"2.15"},{"v":0.408118128,"d":"0.41"}]
["31079","Hall","NE",{"v":1.8567823338491545,"d":"1.86"},{"v":1.8567823338491547,"d":"1.86"},{"v":0.231908258,"d":"0.23"}]
["31081","Hamilton","NE",{"v":1.6903849782206064,"d":"1.69"},{"v":1.6903849782206068,"d":"1.69"},{"v":0.289385122,"d":"0.29"}]
["31083","Harlan","NE",{"v":1.8751035799126299,"d":"1.88"},{"v":1.8751035799126303,"d":"1.88"},{"v":0.305836912,"d":"0.31"}]
["31085","Hayes","NE",{"v":2.1597579537011766,"d":"2.16"},{"v":2.1597579537011766,"d":"2.16"},{"v":0.435418481,"d":"0.44"}]
["31087","Hitchcock","NE",{"v":2.1570940389321738,"d":"2.16"},{"v":2.1570940389321733,"d":"2.16"},{"v":0.43714299,"d":"0.44"}]
["31089","Holt","NE",{"v":1.8518520485880332,"d":"1.85"},{"v":1.8518520485880328,"d":"1.85"},{"v":0.379526902,"d":"0.38"}]
["31091","Hooker","NE",{"v":1.9308446776897332,"d":"1.93"},{"v":1.9308446776897332,"d":"1.93"},{"v":0.54901836,"d":"0.55"}]
["31093","Howard","NE",{"v":1.8345823341088843,"d":"1.83"},{"v":1.834582334108884,"d":"1.83"},{"v":0.418037408,"d":"0.42"}]
["31095","Jefferson","NE",{"v":2.0746636153166893,"d":"2.07"},{"v":2.074663615316689,"d":"2.07"},{"v":0.290468654,"d":"0.29"}]
["31097","Johnson","NE",{"v":2.0939906649887052,"d":"2.09"},{"v":2.0939906649887052,"d":"2.09"},{"v":0.357792063,"d":"0.36"}]
["31099","Kearney","NE",{"v":2.0283979978648787,"d":"2.03"},{"v":2.0283979978648787,"d":"2.03"},{"v":0.255584365,"d":"0.26"}]
["31101","Keith","NE",{"v":2.0937529161982886,"d":"2.09"},{"v":2.093752916198289,"d":"2.09"},{"v":0.283882946,"d":"0.28"}]
["31103","Keya Paha","NE",{"v":1.5793622148063815,"d":"1.58"},{"v":1.5793622148063813,"d":"1.58"},{"v":0.574153217,"d":"0.57"}]
["31105","Kimball","NE",{"v":1.9736692648326921,"d":"1.97"},{"v":1.9736692648326923,"d":"1.97"},{"v":0.328058015,"d":"0.33"}]
["31107","Knox","NE",{"v":2.0973337152703193,"d":"2.10"},{"v":2.0973337152703193,"d":"2.10"},{"v":0.491976842,"d":"0.49"}]
["31109","Lancaster","NE",{"v":1.910578098579948,"d":"1.91"},{"v":1.9105780985799483,"d":"1.91"},{"v":0.271661379,"d":"0.27"}]
["31111","Lincoln","NE",{"v":1.8884942233217348,"d":"1.89"},{"v":1.8884942233217346,"d":"1.89"},{"v":0.237886843,"d":"0.24"}]
["31113","Logan","NE",{"v":2.2302242205562677,"d":"2.23"},{"v":2.230224220556268,"d":"2.23"},{"v":0.541063265,"d":"0.54"}]
["31115","Loup","NE",{"v":2.2460369035217203,"d":"2.25"},{"v":2.2460369035217203,"d":"2.25"},{"v":0.559254676,"d":"0.56"}]
["31117","McPherson","NE",{"v":2.1993219037477294,"d":"2.20"},{"v":2.19932190374773,"d":"2.20"},{"v":0.53083018,"d":"0.53"}]
["31119","Madison","NE",{"v":1.9748008762368947,"d":"1.97"},{"v":1.9748008762368945,"d":"1.97"},{"v":0.315056966,"d":"0.32"}]
["31121","Merrick","NE",{"v":2.1064124515460083,"d":"2.11"},{"v":2.106412451546008,"d":"2.11"},{"v":0.331629155,"d":"0.33"}]
["31123","Morrill","NE",{"v":1.5546677334873293,"d":"1.55"},{"v":1.5546677334873293,"d":"1.55"},{"v":0.3670848950000001,"d":"0.37"}]
["31125","Nance","NE",{"v":2.117280473726915,"d":"2.12"},{"v":2.1172804737269155,"d":"2.12"},{"v":0.384696084,"d":"0.38"}]
["31127","Nemaha","NE",{"v":1.8081535529274966,"d":"1.81"},{"v":1.8081535529274966,"d":"1.81"},{"v":0.30077985699999993,"d":"0.30"}]
["31129","Nuckolls","NE",{"v":2.0410473890071104,"d":"2.04"},{"v":2.04104738900711,"d":"2.04"},{"v":0.304541315,"d":"0.30"}]
["31131","Otoe","NE",{"v":1.9536814728878702,"d":"1.95"},{"v":1.9536814728878706,"d":"1.95"},{"v":0.281705964,"d":"0.28"}]
["31133","Pawnee","NE",{"v":1.9461511210693871,"d":"1.95"},{"v":1.9461511210693874,"d":"1.95"},{"v":0.366493964,"d":"0.37"}]
["31135","Perkins","NE",{"v":2.0846627578641463,"d":"2.08"},{"v":2.084662757864147,"d":"2.08"},{"v":0.342404285,"d":"0.34"}]
["31137","Phelps","NE",{"v":1.553190982734118,"d":"1.55"},{"v":1.553190982734118,"d":"1.55"},{"v":0.238009664,"d":"0.24"}]
["31139","Pierce","NE",{"v":2.1769645519134824,"d":"2.18"},{"v":2.1769645519134824,"d":"2.18"},{"v":0.443669902,"d":"0.44"}]
["31141","Platte","NE",{"v":2.007643800898181,"d":"2.01"},{"v":2.007643800898181,"d":"2.01"},{"v":0.315624965,"d":"0.32"}]
["31143","Polk","NE",{"v":1.9793565469497971,"d":"1.98"},{"v":1.9793565469497971,"d":"1.98"},{"v":0.368422587,"d":"0.37"}]
["31145","Red Willow","NE",{"v":1.9101507142433707,"d":"1.91"},{"v":1.9101507142433707,"d":"1.91"},{"v":0.23181936800000003,"d":"0.23"}]
["31147","Richardson","NE",{"v":2.0668323603701424,"d":"2.07"},{"v":2.0668323603701424,"d":"2.07"},{"v":0.278687836,"d":"0.28"}]
["31149","Rock","NE",{"v":2.17967344123985,"d":"2.18"},{"v":2.17967344123985,"d":"2.18"},{"v":0.442563304,"d":"0.44"}]
["31151","Saline","NE",{"v":1.8871986140782893,"d":"1.89"},{"v":1.887198614078289,"d":"1.89"},{"v":0.275006803,"d":"0.28"}]
["31153","Sarpy","NE",{"v":1.7174691369738266,"d":"1.72"},{"v":1.7174691369738266,"d":"1.72"},{"v":0.309061844,"d":"0.31"}]
["31155","Saunders","NE",{"v":2.1561993030273423,"d":"2.16"},{"v":2.1561993030273428,"d":"2.16"},{"v":0.371523293,"d":"0.37"}]
["31157","Scotts Bluff","NE",{"v":1.9698752123206928,"d":"1.97"},{"v":1.9698752123206928,"d":"1.97"},{"v":0.273117358,"d":"0.27"}]
["31159","Seward","NE",{"v":1.947747184129085,"d":"1.95"},{"v":1.947747184129085,"d":"1.95"},{"v":0.331910186,"d":"0.33"}]
["31161","Sheridan","NE",{"v":2.1446428867072616,"d":"2.14"},{"v":2.144642886707262,"d":"2.14"},{"v":0.384684388,"d":"0.38"}]
["31163","Sherman","NE",{"v":2.15942738407629,"d":"2.16"},{"v":2.15942738407629,"d":"2.16"},{"v":0.402121352,"d":"0.40"}]
["31165","Sioux","NE",{"v":2.2081525559255044,"d":"2.21"},{"v":2.2081525559255044,"d":"2.21"},{"v":0.503000301,"d":"0.50"}]
["31167","Stanton","NE",{"v":1.8722301507453323,"d":"1.87"},{"v":1.8722301507453323,"d":"1.87"},{"v":0.430907346,"d":"0.43"}]
["31169","Thayer","NE",{"v":1.9639688496403076,"d":"1.96"},{"v":1.963968849640308,"d":"1.96"},{"v":0.321659939,"d":"0.32"}]
["31171","Thomas","NE",{"v":2.22386018338332,"d":"2.22"},{"v":2.22386018338332,"d":"2.22"},{"v":0.525578402,"d":"0.53"}]
["31173","Thurston","NE",{"v":2.145225737650057,"d":"2.15"},{"v":2.1452257376500565,"d":"2.15"},{"v":0.464906644,"d":"0.46"}]
["31175","Valley","NE",{"v":2.1475921164495655,"d":"2.15"},{"v":2.147592116449565,"d":"2.15"},{"v":0.405859249,"d":"0.41"}]
["31177","Washington","NE",{"v":1.8433190989191512,"d":"1.84"},{"v":1.8433190989191512,"d":"1.84"},{"v":0.360660171,"d":"0.36"}]
["31179","Wayne","NE",{"v":2.1347749208237246,"d":"2.13"},{"v":2.134774920823725,"d":"2.13"},{"v":0.370362106,"d":"0.37"}]
["31181","Webster","NE",{"v":1.6419858907211855,"d":"1.64"},{"v":1.6419858907211855,"d":"1.64"},{"v":0.301797247,"d":"0.30"}]
["31183","Wheeler","NE",{"v":2.2471861935269155,"d":"2.25"},{"v":2.247186193526916,"d":"2.25"},{"v":0.554716497,"d":"0.55"}]
["31185","York","NE",{"v":2.0751117753453703,"d":"2.08"},{"v":2.07511177534537,"d":"2.08"},{"v":0.295847356,"d":"0.30"}]
["32001","Churchill","NV",{"v":1.6404822393826268,"d":"1.64"},{"v":1.6404822393826273,"d":"1.64"},{"v":0.205654011,"d":"0.21"}]
["32003","Clark","NV",{"v":1.3435341057785326,"d":"1.34"},{"v":1.3435341057785326,"d":"1.34"},{"v":0.06913165,"d":"0.07"}]
["32005","Douglas","NV",{"v":1.5931466393232256,"d":"1.59"},{"v":1.5931466393232256,"d":"1.59"},{"v":0.211167283,"d":"0.21"}]
["32007","Elko","NV",{"v":1.7723127657898428,"d":"1.77"},{"v":1.7723127657898428,"d":"1.77"},{"v":0.35281094,"d":"0.35"}]
["32009","Esmeralda","NV",{"v":1.7554504849806383,"d":"1.76"},{"v":1.7554504849806378,"d":"1.76"},{"v":0.323458384,"d":"0.32"}]
["32011","Eureka","NV",{"v":1.853053801089126,"d":"1.85"},{"v":1.8530538010891258,"d":"1.85"},{"v":0.575964323,"d":"0.58"}]
["32013","Humboldt","NV",{"v":1.6985151880229084,"d":"1.70"},{"v":1.6985151880229086,"d":"1.70"},{"v":0.22196903999999998,"d":"0.22"}]
["32015","Lander","NV",{"v":1.8186456894915402,"d":"1.82"},{"v":1.8186456894915404,"d":"1.82"},{"v":0.34156688800000007,"d":"0.34"}]
["32017","Lincoln","NV",{"v":1.7190400046379108,"d":"1.72"},{"v":1.7190400046379108,"d":"1.72"},{"v":0.337643762,"d":"0.34"}]
["32019","Lyon","NV",{"v":1.6332542335458828,"d":"1.63"},{"v":1.6332542335458828,"d":"1.63"},{"v":0.210528981,"d":"0.21"}]
["32021","Mineral","NV",{"v":1.6649998999579256,"d":"1.66"},{"v":1.6649998999579256,"d":"1.66"},{"v":0.247524844,"d":"0.25"}]
["32023","Nye","NV",{"v":1.7110519080501636,"d":"1.71"},{"v":1.7110519080501636,"d":"1.71"},{"v":0.265276608,"d":"0.27"}]
["32027","Pershing","NV",{"v":1.7438925307238171,"d":"1.74"},{"v":1.7438925307238167,"d":"1.74"},{"v":0.306433634,"d":"0.31"}]
["32029","Storey","NV",{"v":1.7273949983911798,"d":"1.73"},{"v":1.72739499839118,"d":"1.73"},{"v":0.32114167,"d":"0.32"}]
["32031","Washoe","NV",{"v":1.6063026426062603,"d":"1.61"},{"v":1.6063026426062603,"d":"1.61"},{"v":0.161177295,"d":"0.16"}]
["32033","White Pine","NV",{"v":1.8293830457906686,"d":"1.83"},{"v":1.8293830457906688,"d":"1.83"},{"v":0.500775246,"d":"0.50"}]
["32510","Carson City","NV",{"v":1.5115374906408783,"d":"1.51"},{"v":1.5115374906408785,"d":"1.51"},{"v":0.20241949700000003,"d":"0.20"}]
["33001","Belknap","NH",{"v":4.373674837197823,"d":"4.37"},{"v":4.373674837197824,"d":"4.37"},{"v":2.159490999,"d":"2.16"}]
["33003","Carroll","NH",{"v":4.857659216728904,"d":"4.86"},{"v":4.857659216728904,"d":"4.86"},{"v":2.704522549,"d":"2.70"}]
["33005","Cheshire","NH",{"v":4.517759958965768,"d":"4.52"},{"v":4.517759958965768,"d":"4.52"},{"v":2.712570239,"d":"2.71"}]
["33007","Coos","NH",{"v":4.789511881746687,"d":"4.79"},{"v":4.789511881746687,"d":"4.79"},{"v":4.044255186,"d":"4.04"}]
["33009","Grafton","NH",{"v":4.993541303285658,"d":"4.99"},{"v":4.993541303285659,"d":"4.99"},{"v":4.193245556,"d":"4.19"}]
["33011","Hillsborough","NH",{"v":3.9881784316386777,"d":"3.99"},{"v":3.9881784316386777,"d":"3.99"},{"v":1.837046179,"d":"1.84"}]
["33013","Merrimack","NH",{"v":4.223291582731492,"d":"4.22"},{"v":4.223291582731492,"d":"4.22"},{"v":2.094343326,"d":"2.09"}]
["33015","Rockingham","NH",{"v":4.182835754088067,"d":"4.18"},{"v":4.182835754088067,"d":"4.18"},{"v":1.91310901,"d":"1.91"}]
["33017","Strafford","NH",{"v":4.036189406425662,"d":"4.04"},{"v":4.036189406425662,"d":"4.04"},{"v":2.015769979,"d":"2.02"}]
["33019","Sullivan","NH",{"v":4.436449269692577,"d":"4.44"},{"v":4.436449269692578,"d":"4.44"},{"v":2.615273229,"d":"2.62"}]
["34001","Atlantic","NJ",{"v":3.076946569715378,"d":"3.08"},{"v":3.076946569715378,"d":"3.08"},{"v":0.443310061,"d":"0.44"}]
["34003","Bergen","NJ",{"v":2.0929047636427455E-4,"d":"0.00"},{"v":2.0929047636427457E-4,"d":"0.00"},{"v":3.750708072,"d":"3.75"}]
["34005","Burlington","NJ",{"v":3.4044648764123657,"d":"3.40"},{"v":3.4044648764123653,"d":"3.40"},{"v":0.513958713,"d":"0.51"}]
["34007","Camden","NJ",{"v":0.11154761048975328,"d":"0.11"},{"v":0.11154761048975328,"d":"0.11"},{"v":1.119130219,"d":"1.12"}]
["34009","Cape May","NJ",{"v":3.234241697893579,"d":"3.23"},{"v":3.2342416978935793,"d":"3.23"},{"v":0.33961525400000003,"d":"0.34"}]
["34011","Cumberland","NJ",{"v":3.217579644599774,"d":"3.22"},{"v":3.2175796445997746,"d":"3.22"},{"v":0.416014034,"d":"0.42"}]
["34013","Essex","NJ",{"v":9.4247886777013585E-8,"d":"0.00"},{"v":9.4247886777013585E-8,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["34015","Gloucester","NJ",{"v":2.731001565207406,"d":"2.73"},{"v":2.731001565207406,"d":"2.73"},{"v":0.50286639,"d":"0.50"}]
["34017","Hudson","NJ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["34019","Hunterdon","NJ",{"v":3.6308098009010363,"d":"3.63"},{"v":3.6308098009010363,"d":"3.63"},{"v":0.777300901,"d":"0.78"}]
["34021","Mercer","NJ",{"v":1.0886886924593608,"d":"1.09"},{"v":1.0886886924593606,"d":"1.09"},{"v":0.736479203,"d":"0.74"}]
["34023","Middlesex","NJ",{"v":0.04850653455927625,"d":"0.05"},{"v":0.04850653455927625,"d":"0.05"},{"v":1.229450059,"d":"1.23"}]
["34025","Monmouth","NJ",{"v":1.6928975440348046,"d":"1.69"},{"v":1.6928975440348046,"d":"1.69"},{"v":0.531268285,"d":"0.53"}]
["34027","Morris","NJ",{"v":2.5651568221256213,"d":"2.57"},{"v":2.5651568221256213,"d":"2.57"},{"v":0.997575722,"d":"1.00"}]
["34029","Ocean","NJ",{"v":2.741102251119517,"d":"2.74"},{"v":2.741102251119517,"d":"2.74"},{"v":0.423572501,"d":"0.42"}]
["34031","Passaic","NJ",{"v":0.04769715638138104,"d":"0.05"},{"v":0.047697156381381035,"d":"0.05"},{"v":2.409575804,"d":"2.41"}]
["34033","Salem","NJ",{"v":3.3987443443998533,"d":"3.40"},{"v":3.398744344399853,"d":"3.40"},{"v":0.449623164,"d":"0.45"}]
["34035","Somerset","NJ",{"v":2.4138725916310624,"d":"2.41"},{"v":2.4138725916310624,"d":"2.41"},{"v":0.72692306,"d":"0.73"}]
["34037","Sussex","NJ",{"v":3.985780882920629,"d":"3.99"},{"v":3.9857808829206296,"d":"3.99"},{"v":1.14135254,"d":"1.14"}]
["34039","Union","NJ",{"v":5.043916223765203E-6,"d":"0.00"},{"v":5.043916223765203E-6,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["34041","Warren","NJ",{"v":3.7837676893606904,"d":"3.78"},{"v":3.78376768936069,"d":"3.78"},{"v":0.862805384,"d":"0.86"}]
["35001","Bernalillo","NM",{"v":4.596116986784808,"d":"4.60"},{"v":4.596116986784808,"d":"4.60"},{"v":0.441500903,"d":"0.44"}]
["35003","Catron","NM",{"v":6.19774164198582,"d":"6.20"},{"v":6.197741641985821,"d":"6.20"},{"v":1.486352461,"d":"1.49"}]
["35005","Chaves","NM",{"v":5.044240110990074,"d":"5.04"},{"v":5.044240110990074,"d":"5.04"},{"v":0.37947761399999996,"d":"0.38"}]
["35006","Cibola","NM",{"v":5.733577722574463,"d":"5.73"},{"v":5.733577722574462,"d":"5.73"},{"v":0.854299924,"d":"0.85"}]
["35007","Colfax","NM",{"v":5.853338247185155,"d":"5.85"},{"v":5.853338247185155,"d":"5.85"},{"v":1.064267623,"d":"1.06"}]
["35009","Curry","NM",{"v":5.319845953888042,"d":"5.32"},{"v":5.319845953888043,"d":"5.32"},{"v":0.451100268,"d":"0.45"}]
["35011","De Baca","NM",{"v":5.155237339119281,"d":"5.16"},{"v":5.15523733911928,"d":"5.16"},{"v":0.497346658,"d":"0.50"}]
["35013","Dona Ana","NM",{"v":4.829713115791556,"d":"4.83"},{"v":4.829713115791557,"d":"4.83"},{"v":0.3000617380000001,"d":"0.30"}]
["35015","Eddy","NM",{"v":5.0413228939088315,"d":"5.04"},{"v":5.041322893908831,"d":"5.04"},{"v":0.38053509,"d":"0.38"}]
["35017","Grant","NM",{"v":5.25243432629117,"d":"5.25"},{"v":5.25243432629117,"d":"5.25"},{"v":0.44417421399999996,"d":"0.44"}]
["35019","Guadalupe","NM",{"v":5.466478079695319,"d":"5.47"},{"v":5.466478079695319,"d":"5.47"},{"v":0.582979189,"d":"0.58"}]
["35021","Harding","NM",{"v":5.707419403674266,"d":"5.71"},{"v":5.707419403674267,"d":"5.71"},{"v":0.8675129199999999,"d":"0.87"}]
["35023","Hidalgo","NM",{"v":5.387696556033684,"d":"5.39"},{"v":5.387696556033684,"d":"5.39"},{"v":0.470407434,"d":"0.47"}]
["35025","Lea","NM",{"v":5.161758189244019,"d":"5.16"},{"v":5.161758189244019,"d":"5.16"},{"v":0.374506237,"d":"0.37"}]
["35027","Lincoln","NM",{"v":5.446607819486581,"d":"5.45"},{"v":5.446607819486581,"d":"5.45"},{"v":0.661200435,"d":"0.66"}]
["35028","Los Alamos","NM",{"v":5.480453033212044,"d":"5.48"},{"v":5.480453033212044,"d":"5.48"},{"v":0.852368283,"d":"0.85"}]
["35029","Luna","NM",{"v":5.16266317792562,"d":"5.16"},{"v":5.16266317792562,"d":"5.16"},{"v":0.374339097,"d":"0.37"}]
["35031","Mckinley","NM",{"v":5.825860692833176,"d":"5.83"},{"v":5.825860692833177,"d":"5.83"},{"v":0.9657221480000001,"d":"0.97"}]
["35033","Mora","NM",{"v":6.268417845568691,"d":"6.27"},{"v":6.26841784556869,"d":"6.27"},{"v":1.786093327,"d":"1.79"}]
["35035","Otero","NM",{"v":5.56817401637518,"d":"5.57"},{"v":5.56817401637518,"d":"5.57"},{"v":0.654087209,"d":"0.65"}]
["35037","Quay","NM",{"v":5.481586248555023,"d":"5.48"},{"v":5.481586248555022,"d":"5.48"},{"v":0.593345938,"d":"0.59"}]
["35039","Rio Arriba","NM",{"v":5.94692652755303,"d":"5.95"},{"v":5.94692652755303,"d":"5.95"},{"v":1.108346001,"d":"1.11"}]
["35041","Roosevelt","NM",{"v":5.4040607447681195,"d":"5.40"},{"v":5.4040607447681195,"d":"5.40"},{"v":0.562996653,"d":"0.56"}]
["35043","Sandoval","NM",{"v":5.638797786035029,"d":"5.64"},{"v":5.63879778603503,"d":"5.64"},{"v":0.743380185,"d":"0.74"}]
["35045","San Juan","NM",{"v":5.776963668623367,"d":"5.78"},{"v":5.776963668623366,"d":"5.78"},{"v":0.715280513,"d":"0.72"}]
["35047","San Miguel","NM",{"v":6.081047246963933,"d":"6.08"},{"v":6.081047246963934,"d":"6.08"},{"v":1.262390631,"d":"1.26"}]
["35049","Santa Fe","NM",{"v":5.662026968527246,"d":"5.66"},{"v":5.662026968527245,"d":"5.66"},{"v":0.857899947,"d":"0.86"}]
["35051","Sierra","NM",{"v":5.2013210477835745,"d":"5.20"},{"v":5.2013210477835745,"d":"5.20"},{"v":0.356624204,"d":"0.36"}]
["35053","Socorro","NM",{"v":5.3606703340522355,"d":"5.36"},{"v":5.360670334052235,"d":"5.36"},{"v":0.541374647,"d":"0.54"}]
["35055","Taos","NM",{"v":5.965476037902484,"d":"5.97"},{"v":5.965476037902484,"d":"5.97"},{"v":1.346440506,"d":"1.35"}]
["35057","Torrance","NM",{"v":5.68466913238808,"d":"5.68"},{"v":5.6846691323880805,"d":"5.68"},{"v":0.8129905310000001,"d":"0.81"}]
["35059","Union","NM",{"v":5.299030473165006,"d":"5.30"},{"v":5.299030473165006,"d":"5.30"},{"v":0.633547261,"d":"0.63"}]
["35061","Valencia","NM",{"v":5.088204341146694,"d":"5.09"},{"v":5.088204341146695,"d":"5.09"},{"v":0.371180123,"d":"0.37"}]
["36001","Albany","NY",{"v":1.5897704485643327,"d":"1.59"},{"v":1.5897704485643327,"d":"1.59"},{"v":0.45848866399999993,"d":"0.46"}]
["36003","Allegany","NY",{"v":2.0526060546920375,"d":"2.05"},{"v":2.052606054692037,"d":"2.05"},{"v":0.651333804,"d":"0.65"}]
["36005","Bronx","NY",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["36007","Broome","NY",{"v":1.8081753915882326,"d":"1.81"},{"v":1.8081753915882328,"d":"1.81"},{"v":0.58082942,"d":"0.58"}]
["36009","Cattaraugus","NY",{"v":2.0374736174829957,"d":"2.04"},{"v":2.0374736174829957,"d":"2.04"},{"v":0.648055786,"d":"0.65"}]
["36011","Cayuga","NY",{"v":1.826998027904099,"d":"1.83"},{"v":1.826998027904099,"d":"1.83"},{"v":0.428879193,"d":"0.43"}]
["36013","Chautauqua","NY",{"v":1.8665133844413013,"d":"1.87"},{"v":1.8665133844413013,"d":"1.87"},{"v":0.415281056,"d":"0.42"}]
["36015","Chemung","NY",{"v":1.7894542486880873,"d":"1.79"},{"v":1.7894542486880873,"d":"1.79"},{"v":0.477892213,"d":"0.48"}]
["36017","Chenango","NY",{"v":2.079503015578669,"d":"2.08"},{"v":2.0795030155786685,"d":"2.08"},{"v":0.926421748,"d":"0.93"}]
["36019","Clinton","NY",{"v":2.1275342356169724,"d":"2.13"},{"v":2.1275342356169724,"d":"2.13"},{"v":1.112841878,"d":"1.11"}]
["36021","Columbia","NY",{"v":2.0286222611219964,"d":"2.03"},{"v":2.0286222611219964,"d":"2.03"},{"v":0.69958341,"d":"0.70"}]
["36023","Cortland","NY",{"v":1.8726653201658607,"d":"1.87"},{"v":1.872665320165861,"d":"1.87"},{"v":0.585030689,"d":"0.59"}]
["36025","Delaware","NY",{"v":2.11881009170668,"d":"2.12"},{"v":2.11881009170668,"d":"2.12"},{"v":1.064569366,"d":"1.06"}]
["36027","Dutchess","NY",{"v":1.9309914160474397,"d":"1.93"},{"v":1.93099141604744,"d":"1.93"},{"v":0.612015149,"d":"0.61"}]
["36029","Erie","NY",{"v":1.2361546715223568,"d":"1.24"},{"v":1.2361546715223568,"d":"1.24"},{"v":0.410630878,"d":"0.41"}]
["36031","Essex","NY",{"v":2.2802332383754553,"d":"2.28"},{"v":2.280233238375455,"d":"2.28"},{"v":1.522562883,"d":"1.52"}]
["36033","Franklin","NY",{"v":2.1517258368136676,"d":"2.15"},{"v":2.1517258368136676,"d":"2.15"},{"v":1.191372255,"d":"1.19"}]
["36035","Fulton","NY",{"v":1.9295063710437528,"d":"1.93"},{"v":1.929506371043753,"d":"1.93"},{"v":0.8278142010000001,"d":"0.83"}]
["36037","Genesee","NY",{"v":1.7877838257253333,"d":"1.79"},{"v":1.7877838257253333,"d":"1.79"},{"v":0.426157687,"d":"0.43"}]
["36039","Greene","NY",{"v":2.1854796750203622,"d":"2.19"},{"v":2.185479675020362,"d":"2.19"},{"v":1.1675026,"d":"1.17"}]
["36041","Hamilton","NY",{"v":2.393620756836085,"d":"2.39"},{"v":2.393620756836085,"d":"2.39"},{"v":1.886829552,"d":"1.89"}]
["36043","Herkimer","NY",{"v":2.0899056849105033,"d":"2.09"},{"v":2.0899056849105033,"d":"2.09"},{"v":1.047085551,"d":"1.05"}]
["36045","Jefferson","NY",{"v":1.8966816462169593,"d":"1.90"},{"v":1.8966816462169593,"d":"1.90"},{"v":0.412169567,"d":"0.41"}]
["36047","Kings","NY",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["36049","Lewis","NY",{"v":2.225957168959987,"d":"2.23"},{"v":2.225957168959987,"d":"2.23"},{"v":1.374175779,"d":"1.37"}]
["36051","Livingston","NY",{"v":1.8541319796004037,"d":"1.85"},{"v":1.8541319796004037,"d":"1.85"},{"v":0.46420879,"d":"0.46"}]
["36053","Madison","NY",{"v":1.899721923586117,"d":"1.90"},{"v":1.8997219235861171,"d":"1.90"},{"v":0.582492969,"d":"0.58"}]
["36055","Monroe","NY",{"v":1.042905433075747,"d":"1.04"},{"v":1.0429054330757472,"d":"1.04"},{"v":0.440913229,"d":"0.44"}]
["36057","Montgomery","NY",{"v":1.8651308469561734,"d":"1.87"},{"v":1.8651308469561734,"d":"1.87"},{"v":0.555044359,"d":"0.56"}]
["36059","Nassau","NY",{"v":4.0789946448630763E-5,"d":"0.00"},{"v":4.0789946448630763E-5,"d":"0.00"},{"v":2.012168777,"d":"2.01"}]
["36061","New York","NY",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["36063","Niagara","NY",{"v":1.6471930821715703,"d":"1.65"},{"v":1.6471930821715703,"d":"1.65"},{"v":0.306596845,"d":"0.31"}]
["36065","Oneida","NY",{"v":1.8104547130077557,"d":"1.81"},{"v":1.8104547130077557,"d":"1.81"},{"v":0.556770648,"d":"0.56"}]
["36067","Onondaga","NY",{"v":1.6260598425255564,"d":"1.63"},{"v":1.6260598425255561,"d":"1.63"},{"v":0.41052325,"d":"0.41"}]
["36069","Ontario","NY",{"v":1.8304105283508294,"d":"1.83"},{"v":1.8304105283508292,"d":"1.83"},{"v":0.405024689,"d":"0.41"}]
["36071","Orange","NY",{"v":1.8583398758202918,"d":"1.86"},{"v":1.8583398758202916,"d":"1.86"},{"v":0.542370708,"d":"0.54"}]
["36073","Orleans","NY",{"v":1.8428915891177133,"d":"1.84"},{"v":1.8428915891177133,"d":"1.84"},{"v":0.422983088,"d":"0.42"}]
["36075","Oswego","NY",{"v":1.8741312084188266,"d":"1.87"},{"v":1.8741312084188269,"d":"1.87"},{"v":0.561516528,"d":"0.56"}]
["36077","Otsego","NY",{"v":2.040151859917128,"d":"2.04"},{"v":2.040151859917128,"d":"2.04"},{"v":0.832257121,"d":"0.83"}]
["36079","Putnam","NY",{"v":1.9991050067615581,"d":"2.00"},{"v":1.999105006761558,"d":"2.00"},{"v":0.748606012,"d":"0.75"}]
["36081","Queens","NY",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["36083","Rensselaer","NY",{"v":1.7939477142455291,"d":"1.79"},{"v":1.793947714245529,"d":"1.79"},{"v":0.50448265,"d":"0.50"}]
["36085","Richmond","NY",{"v":8.450102658825481e-11,"d":"0.00"},{"v":8.450102658825481e-11,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["36087","Rockland","NY",{"v":0.5401893677533169,"d":"0.54"},{"v":0.5401893677533169,"d":"0.54"},{"v":0.748246751,"d":"0.75"}]
["36089","St Lawrence","NY",{"v":2.06681263222907,"d":"2.07"},{"v":2.0668126322290705,"d":"2.07"},{"v":0.846863374,"d":"0.85"}]
["36091","Saratoga","NY",{"v":1.8905531803381934,"d":"1.89"},{"v":1.8905531803381934,"d":"1.89"},{"v":0.531556569,"d":"0.53"}]
["36093","Schenectady","NY",{"v":1.5407990400920493,"d":"1.54"},{"v":1.5407990400920495,"d":"1.54"},{"v":0.46196304600000004,"d":"0.46"}]
["36095","Schoharie","NY",{"v":2.171135697123916,"d":"2.17"},{"v":2.171135697123916,"d":"2.17"},{"v":1.032642432,"d":"1.03"}]
["36097","Schuyler","NY",{"v":2.0300730471970634,"d":"2.03"},{"v":2.030073047197064,"d":"2.03"},{"v":0.70261749,"d":"0.70"}]
["36099","Seneca","NY",{"v":1.8554227485507073,"d":"1.86"},{"v":1.8554227485507073,"d":"1.86"},{"v":0.400216305,"d":"0.40"}]
["36101","Steuben","NY",{"v":2.018959668512561,"d":"2.02"},{"v":2.018959668512561,"d":"2.02"},{"v":0.559826067,"d":"0.56"}]
["36103","Suffolk","NY",{"v":0.6823197072744225,"d":"0.68"},{"v":0.6823197072744226,"d":"0.68"},{"v":0.38177972,"d":"0.38"}]
["36105","Sullivan","NY",{"v":2.1902283181476663,"d":"2.19"},{"v":2.1902283181476663,"d":"2.19"},{"v":1.22372886,"d":"1.22"}]
["36107","Tioga","NY",{"v":2.00874285349226,"d":"2.01"},{"v":2.00874285349226,"d":"2.01"},{"v":0.754740623,"d":"0.75"}]
["36109","Tompkins","NY",{"v":1.8523813078842093,"d":"1.85"},{"v":1.8523813078842093,"d":"1.85"},{"v":0.53254775,"d":"0.53"}]
["36111","Ulster","NY",{"v":2.110138042204676,"d":"2.11"},{"v":2.110138042204676,"d":"2.11"},{"v":1.057163371,"d":"1.06"}]
["36113","Warren","NY",{"v":2.1088096936942216,"d":"2.11"},{"v":2.108809693694221,"d":"2.11"},{"v":1.026328019,"d":"1.03"}]
["36115","Washington","NY",{"v":1.9933775547733958,"d":"1.99"},{"v":1.9933775547733954,"d":"1.99"},{"v":0.604428179,"d":"0.60"}]
["36117","Wayne","NY",{"v":1.8337701096286987,"d":"1.83"},{"v":1.8337701096286987,"d":"1.83"},{"v":0.463556671,"d":"0.46"}]
["36119","Westchester","NY",{"v":0.08262825560969234,"d":"0.08"},{"v":0.08262825560969234,"d":"0.08"},{"v":1.213208688,"d":"1.21"}]
["36121","Wyoming","NY",{"v":1.8526896219391276,"d":"1.85"},{"v":1.8526896219391276,"d":"1.85"},{"v":0.499509081,"d":"0.50"}]
["36123","Yates","NY",{"v":1.9090693592519847,"d":"1.91"},{"v":1.9090693592519847,"d":"1.91"},{"v":0.509840898,"d":"0.51"}]
["37001","Alamance","NC",{"v":1.8012197617261712,"d":"1.80"},{"v":1.801219761726171,"d":"1.80"},{"v":0.304462974,"d":"0.30"}]
["37003","Alexander","NC",{"v":2.0258603070027306,"d":"2.03"},{"v":2.02586030700273,"d":"2.03"},{"v":0.429922045,"d":"0.43"}]
["37005","Alleghany","NC",{"v":1.994283597643167,"d":"1.99"},{"v":1.9942835976431672,"d":"1.99"},{"v":0.620202699,"d":"0.62"}]
["37007","Anson","NC",{"v":2.0694667901084274,"d":"2.07"},{"v":2.0694667901084274,"d":"2.07"},{"v":0.390054937,"d":"0.39"}]
["37009","Ashe","NC",{"v":2.165671896101523,"d":"2.17"},{"v":2.165671896101523,"d":"2.17"},{"v":0.672916497,"d":"0.67"}]
["37011","Avery","NC",{"v":2.0694192597791874,"d":"2.07"},{"v":2.0694192597791874,"d":"2.07"},{"v":0.779969449,"d":"0.78"}]
["37013","Beaufort","NC",{"v":1.8409993820666148,"d":"1.84"},{"v":1.8409993820666148,"d":"1.84"},{"v":0.251555563,"d":"0.25"}]
["37015","Bertie","NC",{"v":1.9403409232651276,"d":"1.94"},{"v":1.9403409232651276,"d":"1.94"},{"v":0.390016118,"d":"0.39"}]
["37017","Bladen","NC",{"v":1.8807137418246527,"d":"1.88"},{"v":1.8807137418246525,"d":"1.88"},{"v":0.34803068099999995,"d":"0.35"}]
["37019","Brunswick","NC",{"v":1.9190254912391704,"d":"1.92"},{"v":1.9190254912391702,"d":"1.92"},{"v":0.259764278,"d":"0.26"}]
["37021","Buncombe","NC",{"v":1.9727204552488011,"d":"1.97"},{"v":1.972720455248801,"d":"1.97"},{"v":0.527139828,"d":"0.53"}]
["37023","Burke","NC",{"v":2.108018951103046,"d":"2.11"},{"v":2.1080189511030456,"d":"2.11"},{"v":0.550267432,"d":"0.55"}]
["37025","Cabarrus","NC",{"v":1.7905733079000778,"d":"1.79"},{"v":1.7905733079000776,"d":"1.79"},{"v":0.258114919,"d":"0.26"}]
["37027","Caldwell","NC",{"v":2.1600681357889218,"d":"2.16"},{"v":2.1600681357889218,"d":"2.16"},{"v":0.563294593,"d":"0.56"}]
["37029","Camden","NC",{"v":1.7961677561877836,"d":"1.80"},{"v":1.7961677561877836,"d":"1.80"},{"v":0.308374871,"d":"0.31"}]
["37031","Carteret","NC",{"v":1.6675094699778008,"d":"1.67"},{"v":1.6675094699778006,"d":"1.67"},{"v":0.171640148,"d":"0.17"}]
["37033","Caswell","NC",{"v":1.9556991755100739,"d":"1.96"},{"v":1.955699175510074,"d":"1.96"},{"v":0.49664747899999995,"d":"0.50"}]
["37035","Catawba","NC",{"v":1.9761349356226778,"d":"1.98"},{"v":1.976134935622678,"d":"1.98"},{"v":0.3137498819999999,"d":"0.31"}]
["37037","Chatham","NC",{"v":1.9179169936025047,"d":"1.92"},{"v":1.9179169936025047,"d":"1.92"},{"v":0.380984437,"d":"0.38"}]
["37039","Cherokee","NC",{"v":2.4167490164721315,"d":"2.42"},{"v":2.4167490164721315,"d":"2.42"},{"v":0.766361526,"d":"0.77"}]
["37041","Chowan","NC",{"v":1.8509168987595712,"d":"1.85"},{"v":1.8509168987595717,"d":"1.85"},{"v":0.25068717,"d":"0.25"}]
["37043","Clay","NC",{"v":2.0180349157810524,"d":"2.02"},{"v":2.0180349157810524,"d":"2.02"},{"v":0.734418669,"d":"0.73"}]
["37045","Cleveland","NC",{"v":2.0203727843038477,"d":"2.02"},{"v":2.0203727843038477,"d":"2.02"},{"v":0.306094207,"d":"0.31"}]
["37047","Columbus","NC",{"v":1.974105274027141,"d":"1.97"},{"v":1.974105274027141,"d":"1.97"},{"v":0.33788428600000003,"d":"0.34"}]
["37049","Craven","NC",{"v":1.8141072972563235,"d":"1.81"},{"v":1.8141072972563237,"d":"1.81"},{"v":0.263915911,"d":"0.26"}]
["37051","Cumberland","NC",{"v":1.5576772670639767,"d":"1.56"},{"v":1.5576772670639767,"d":"1.56"},{"v":0.244984119,"d":"0.24"}]
["37053","Currituck","NC",{"v":1.8453005017333044,"d":"1.85"},{"v":1.8453005017333042,"d":"1.85"},{"v":0.237606926,"d":"0.24"}]
["37055","Dare","NC",{"v":2.3461756258457354,"d":"2.35"},{"v":2.346175625845735,"d":"2.35"},{"v":0.179003202,"d":"0.18"}]
["37057","Davidson","NC",{"v":1.8162278275432304,"d":"1.82"},{"v":1.8162278275432302,"d":"1.82"},{"v":0.374358738,"d":"0.37"}]
["37059","Davie","NC",{"v":2.131660697786031,"d":"2.13"},{"v":2.131660697786031,"d":"2.13"},{"v":0.361921583,"d":"0.36"}]
["37061","Duplin","NC",{"v":1.921055489982448,"d":"1.92"},{"v":1.921055489982448,"d":"1.92"},{"v":0.314405438,"d":"0.31"}]
["37063","Durham","NC",{"v":1.3446567771977715,"d":"1.34"},{"v":1.3446567771977718,"d":"1.34"},{"v":0.433444598,"d":"0.43"}]
["37065","Edgecombe","NC",{"v":1.8344686835377642,"d":"1.83"},{"v":1.8344686835377646,"d":"1.83"},{"v":0.254580323,"d":"0.25"}]
["37067","Forsyth","NC",{"v":1.3018276213624158,"d":"1.30"},{"v":1.3018276213624158,"d":"1.30"},{"v":0.375051868,"d":"0.38"}]
["37069","Franklin","NC",{"v":2.1323804891286335,"d":"2.13"},{"v":2.1323804891286335,"d":"2.13"},{"v":0.476431855,"d":"0.48"}]
["37071","Gaston","NC",{"v":1.6535868042881081,"d":"1.65"},{"v":1.6535868042881083,"d":"1.65"},{"v":0.285270425,"d":"0.29"}]
["37073","Gates","NC",{"v":1.8761905719115743,"d":"1.88"},{"v":1.8761905719115746,"d":"1.88"},{"v":0.410025931,"d":"0.41"}]
["37075","Graham","NC",{"v":2.3666038185654465,"d":"2.37"},{"v":2.3666038185654465,"d":"2.37"},{"v":0.831777211,"d":"0.83"}]
["37077","Granville","NC",{"v":1.9557413603168086,"d":"1.96"},{"v":1.9557413603168083,"d":"1.96"},{"v":0.436871065,"d":"0.44"}]
["37079","Greene","NC",{"v":1.9871211887544147,"d":"1.99"},{"v":1.9871211887544151,"d":"1.99"},{"v":0.282884499,"d":"0.28"}]
["37081","Guilford","NC",{"v":1.3966197560683304,"d":"1.40"},{"v":1.3966197560683302,"d":"1.40"},{"v":0.325319244,"d":"0.33"}]
["37083","Halifax","NC",{"v":1.9039139773472846,"d":"1.90"},{"v":1.9039139773472844,"d":"1.90"},{"v":0.31065843,"d":"0.31"}]
["37085","Harnett","NC",{"v":1.8632113802719068,"d":"1.86"},{"v":1.8632113802719072,"d":"1.86"},{"v":0.292606489,"d":"0.29"}]
["37087","Haywood","NC",{"v":1.9677114594369642,"d":"1.97"},{"v":1.9677114594369638,"d":"1.97"},{"v":0.667322249,"d":"0.67"}]
["37089","Henderson","NC",{"v":2.1221359202110874,"d":"2.12"},{"v":2.1221359202110874,"d":"2.12"},{"v":0.503440607,"d":"0.50"}]
["37091","Hertford","NC",{"v":2.0459459722530506,"d":"2.05"},{"v":2.0459459722530506,"d":"2.05"},{"v":0.347411912,"d":"0.35"}]
["37093","Hoke","NC",{"v":1.8859489984325184,"d":"1.89"},{"v":1.8859489984325188,"d":"1.89"},{"v":0.259895953,"d":"0.26"}]
["37095","Hyde","NC",{"v":1.6781026754020074,"d":"1.68"},{"v":1.6781026754020074,"d":"1.68"},{"v":0.226747892,"d":"0.23"}]
["37097","Iredell","NC",{"v":1.897991709272976,"d":"1.90"},{"v":1.897991709272976,"d":"1.90"},{"v":0.293559852,"d":"0.29"}]
["37099","Jackson","NC",{"v":2.1573008419328112,"d":"2.16"},{"v":2.1573008419328117,"d":"2.16"},{"v":0.74582641,"d":"0.75"}]
["37101","Johnston","NC",{"v":1.8721136242576506,"d":"1.87"},{"v":1.8721136242576508,"d":"1.87"},{"v":0.282304086,"d":"0.28"}]
["37103","Jones","NC",{"v":1.9292545546120596,"d":"1.93"},{"v":1.9292545546120594,"d":"1.93"},{"v":0.372690401,"d":"0.37"}]
["37105","Lee","NC",{"v":1.9870333592042484,"d":"1.99"},{"v":1.9870333592042484,"d":"1.99"},{"v":0.407892405,"d":"0.41"}]
["37107","Lenoir","NC",{"v":1.7955829396656333,"d":"1.80"},{"v":1.7955829396656333,"d":"1.80"},{"v":0.23150207299999997,"d":"0.23"}]
["37109","Lincoln","NC",{"v":1.9583095318537591,"d":"1.96"},{"v":1.9583095318537587,"d":"1.96"},{"v":0.316498321,"d":"0.32"}]
["37111","McDowell","NC",{"v":2.305980810033394,"d":"2.31"},{"v":2.305980810033394,"d":"2.31"},{"v":0.716188199,"d":"0.72"}]
["37113","Macon","NC",{"v":2.3518794604065985,"d":"2.35"},{"v":2.3518794604065985,"d":"2.35"},{"v":0.737782372,"d":"0.74"}]
["37115","Madison","NC",{"v":1.7232240415214775,"d":"1.72"},{"v":1.7232240415214775,"d":"1.72"},{"v":0.716325243,"d":"0.72"}]
["37117","Martin","NC",{"v":1.8741463451438731,"d":"1.87"},{"v":1.8741463451438731,"d":"1.87"},{"v":0.3514213829999999,"d":"0.35"}]
["37119","Mecklenburg","NC",{"v":0.12221455210609748,"d":"0.12"},{"v":0.1222145521060975,"d":"0.12"},{"v":0.447643971,"d":"0.45"}]
["37121","Mitchell","NC",{"v":1.9469602208510206,"d":"1.95"},{"v":1.9469602208510204,"d":"1.95"},{"v":0.726206485,"d":"0.73"}]
["37123","Montgomery","NC",{"v":2.006675644171973,"d":"2.01"},{"v":2.006675644171973,"d":"2.01"},{"v":0.453290372,"d":"0.45"}]
["37125","Moore","NC",{"v":1.9225939429651933,"d":"1.92"},{"v":1.922593942965193,"d":"1.92"},{"v":0.361208074,"d":"0.36"}]
["37127","Nash","NC",{"v":1.7684953777629964,"d":"1.77"},{"v":1.7684953777629966,"d":"1.77"},{"v":0.29193054,"d":"0.29"}]
["37129","New Hanover","NC",{"v":1.0952676964934593,"d":"1.10"},{"v":1.0952676964934591,"d":"1.10"},{"v":0.251307689,"d":"0.25"}]
["37131","Northampton","NC",{"v":2.0938965573331774,"d":"2.09"},{"v":2.093896557333177,"d":"2.09"},{"v":0.372503869,"d":"0.37"}]
["37133","Onslow","NC",{"v":1.9202516270806211,"d":"1.92"},{"v":1.9202516270806211,"d":"1.92"},{"v":0.257314785,"d":"0.26"}]
["37135","Orange","NC",{"v":1.7651835980398585,"d":"1.77"},{"v":1.7651835980398585,"d":"1.77"},{"v":0.382025589,"d":"0.38"}]
["37137","Pamlico","NC",{"v":1.7648450657580217,"d":"1.76"},{"v":1.7648450657580215,"d":"1.76"},{"v":0.266136115,"d":"0.27"}]
["37139","Pasquotank","NC",{"v":1.8944433583010263,"d":"1.89"},{"v":1.8944433583010263,"d":"1.89"},{"v":0.232951533,"d":"0.23"}]
["37141","Pender","NC",{"v":1.9608465082324449,"d":"1.96"},{"v":1.9608465082324447,"d":"1.96"},{"v":0.347594155,"d":"0.35"}]
["37143","Perquimans","NC",{"v":2.107757058765323,"d":"2.11"},{"v":2.1077570587653227,"d":"2.11"},{"v":0.262543529,"d":"0.26"}]
["37145","Person","NC",{"v":1.9744701025218174,"d":"1.97"},{"v":1.9744701025218176,"d":"1.97"},{"v":0.436882906,"d":"0.44"}]
["37147","Pitt","NC",{"v":1.758117138100265,"d":"1.76"},{"v":1.7581171381002647,"d":"1.76"},{"v":0.22500316599999998,"d":"0.23"}]
["37149","Polk","NC",{"v":2.4614984039397068,"d":"2.46"},{"v":2.4614984039397063,"d":"2.46"},{"v":0.635866668,"d":"0.64"}]
["37151","Randolph","NC",{"v":2.1720136715735947,"d":"2.17"},{"v":2.172013671573595,"d":"2.17"},{"v":0.390517994,"d":"0.39"}]
["37153","Richmond","NC",{"v":1.936272328272475,"d":"1.94"},{"v":1.936272328272475,"d":"1.94"},{"v":0.326238017,"d":"0.33"}]
["37155","Robeson","NC",{"v":1.9040300405293884,"d":"1.90"},{"v":1.9040300405293884,"d":"1.90"},{"v":0.269810844,"d":"0.27"}]
["37157","Rockingham","NC",{"v":2.062686628915377,"d":"2.06"},{"v":2.062686628915377,"d":"2.06"},{"v":0.386139409,"d":"0.39"}]
["37159","Rowan","NC",{"v":1.810286539793263,"d":"1.81"},{"v":1.810286539793263,"d":"1.81"},{"v":0.310282178,"d":"0.31"}]
["37161","Rutherford","NC",{"v":2.0041444192217375,"d":"2.00"},{"v":2.004144419221738,"d":"2.00"},{"v":0.548666738,"d":"0.55"}]
["37163","Sampson","NC",{"v":1.9641768356059184,"d":"1.96"},{"v":1.9641768356059186,"d":"1.96"},{"v":0.286954199,"d":"0.29"}]
["37165","Scotland","NC",{"v":1.7154988113614034,"d":"1.72"},{"v":1.715498811361403,"d":"1.72"},{"v":0.255461811,"d":"0.26"}]
["37167","Stanly","NC",{"v":2.0510267989999638,"d":"2.05"},{"v":2.0510267989999638,"d":"2.05"},{"v":0.328111254,"d":"0.33"}]
["37169","Stokes","NC",{"v":2.0365161724547503,"d":"2.04"},{"v":2.0365161724547507,"d":"2.04"},{"v":0.48726190699999994,"d":"0.49"}]
["37171","Surry","NC",{"v":2.1427955842181783,"d":"2.14"},{"v":2.142795584218178,"d":"2.14"},{"v":0.540703071,"d":"0.54"}]
["37173","Swain","NC",{"v":2.5124656726158077,"d":"2.51"},{"v":2.5124656726158077,"d":"2.51"},{"v":0.82765201,"d":"0.83"}]
["37175","Transylvania","NC",{"v":1.9818701021456073,"d":"1.98"},{"v":1.9818701021456075,"d":"1.98"},{"v":0.657031469,"d":"0.66"}]
["37177","Tyrrell","NC",{"v":1.7356755202209804,"d":"1.74"},{"v":1.7356755202209802,"d":"1.74"},{"v":0.340658336,"d":"0.34"}]
["37179","Union","NC",{"v":1.9396599025542371,"d":"1.94"},{"v":1.9396599025542371,"d":"1.94"},{"v":0.22632005199999997,"d":"0.23"}]
["37181","Vance","NC",{"v":1.9118685499734753,"d":"1.91"},{"v":1.9118685499734753,"d":"1.91"},{"v":0.404467272,"d":"0.40"}]
["37183","Wake","NC",{"v":1.0700503416763554,"d":"1.07"},{"v":1.0700503416763554,"d":"1.07"},{"v":0.389016981,"d":"0.39"}]
["37185","Warren","NC",{"v":2.0324633734138033,"d":"2.03"},{"v":2.032463373413803,"d":"2.03"},{"v":0.511311039,"d":"0.51"}]
["37187","Washington","NC",{"v":1.6270932474273225,"d":"1.63"},{"v":1.6270932474273228,"d":"1.63"},{"v":0.271300308,"d":"0.27"}]
["37189","Watauga","NC",{"v":2.0792391410261772,"d":"2.08"},{"v":2.0792391410261777,"d":"2.08"},{"v":0.677581836,"d":"0.68"}]
["37191","Wayne","NC",{"v":1.9916340558645786,"d":"1.99"},{"v":1.9916340558645784,"d":"1.99"},{"v":0.247562962,"d":"0.25"}]
["37193","Wilkes","NC",{"v":2.0661202224937263,"d":"2.07"},{"v":2.0661202224937263,"d":"2.07"},{"v":0.625194904,"d":"0.63"}]
["37195","Wilson","NC",{"v":1.8024699679589167,"d":"1.80"},{"v":1.802469967958917,"d":"1.80"},{"v":0.203657537,"d":"0.20"}]
["37197","Yadkin","NC",{"v":2.307510430929551,"d":"2.31"},{"v":2.307510430929551,"d":"2.31"},{"v":0.512862889,"d":"0.51"}]
["37199","Yancey","NC",{"v":2.2233538911934594,"d":"2.22"},{"v":2.2233538911934594,"d":"2.22"},{"v":0.777271363,"d":"0.78"}]
["38001","Adams","ND",{"v":0.5570877071418034,"d":"0.56"},{"v":0.5570877071418034,"d":"0.56"},{"v":0.19190202600000003,"d":"0.19"}]
["38003","Barnes","ND",{"v":0.5590410111675117,"d":"0.56"},{"v":0.5590410111675117,"d":"0.56"},{"v":0.155878295,"d":"0.16"}]
["38005","Benson","ND",{"v":0.5329684419827474,"d":"0.53"},{"v":0.5329684419827474,"d":"0.53"},{"v":0.271200646,"d":"0.27"}]
["38007","Billings","ND",{"v":0.5637615612169578,"d":"0.56"},{"v":0.5637615612169578,"d":"0.56"},{"v":0.21493518599999997,"d":"0.21"}]
["38009","Bottineau","ND",{"v":0.5303022981984867,"d":"0.53"},{"v":0.5303022981984867,"d":"0.53"},{"v":0.282841702,"d":"0.28"}]
["38011","Bowman","ND",{"v":0.5476513794778533,"d":"0.55"},{"v":0.5476513794778533,"d":"0.55"},{"v":0.154911651,"d":"0.15"}]
["38013","Burke","ND",{"v":0.5295198037042568,"d":"0.53"},{"v":0.5295198037042569,"d":"0.53"},{"v":0.252609302,"d":"0.25"}]
["38015","Burleigh","ND",{"v":0.53041776084818,"d":"0.53"},{"v":0.53041776084818,"d":"0.53"},{"v":0.102457115,"d":"0.10"}]
["38017","Cass","ND",{"v":0.505379782007394,"d":"0.51"},{"v":0.505379782007394,"d":"0.51"},{"v":0.131869083,"d":"0.13"}]
["38019","Cavalier","ND",{"v":0.5730770547945908,"d":"0.57"},{"v":0.5730770547945909,"d":"0.57"},{"v":0.22782177399999998,"d":"0.23"}]
["38021","Dickey","ND",{"v":0.5089705974592668,"d":"0.51"},{"v":0.5089705974592666,"d":"0.51"},{"v":0.220642511,"d":"0.22"}]
["38023","Divide","ND",{"v":0.5489344311174784,"d":"0.55"},{"v":0.5489344311174784,"d":"0.55"},{"v":0.25951924,"d":"0.26"}]
["38025","Dunn","ND",{"v":0.5706296510028777,"d":"0.57"},{"v":0.5706296510028778,"d":"0.57"},{"v":0.22973929,"d":"0.23"}]
["38027","Eddy","ND",{"v":0.5596180367579144,"d":"0.56"},{"v":0.5596180367579144,"d":"0.56"},{"v":0.17730215399999996,"d":"0.18"}]
["38029","Emmons","ND",{"v":0.5615545060203869,"d":"0.56"},{"v":0.5615545060203869,"d":"0.56"},{"v":0.191905558,"d":"0.19"}]
["38031","Foster","ND",{"v":0.511346738021529,"d":"0.51"},{"v":0.5113467380215289,"d":"0.51"},{"v":0.192997581,"d":"0.19"}]
["38033","Golden Valley","ND",{"v":0.5392465257586538,"d":"0.54"},{"v":0.5392465257586538,"d":"0.54"},{"v":0.143116766,"d":"0.14"}]
["38035","Grand Forks","ND",{"v":0.49372361874271464,"d":"0.49"},{"v":0.4937236187427146,"d":"0.49"},{"v":0.158573961,"d":"0.16"}]
["38037","Grant","ND",{"v":0.5642227034359026,"d":"0.56"},{"v":0.5642227034359026,"d":"0.56"},{"v":0.217005614,"d":"0.22"}]
["38039","Griggs","ND",{"v":0.5697131694632626,"d":"0.57"},{"v":0.5697131694632626,"d":"0.57"},{"v":0.24784224,"d":"0.25"}]
["38041","Hettinger","ND",{"v":0.5204479425647978,"d":"0.52"},{"v":0.5204479425647979,"d":"0.52"},{"v":0.147925064,"d":"0.15"}]
["38043","Kidder","ND",{"v":0.40384465079790327,"d":"0.40"},{"v":0.40384465079790327,"d":"0.40"},{"v":0.193922094,"d":"0.19"}]
["38045","Lamoure","ND",{"v":0.4851732524904281,"d":"0.49"},{"v":0.4851732524904281,"d":"0.49"},{"v":0.22330321,"d":"0.22"}]
["38047","Logan","ND",{"v":0.5640198985001172,"d":"0.56"},{"v":0.5640198985001172,"d":"0.56"},{"v":0.218241255,"d":"0.22"}]
["38049","McHenry","ND",{"v":0.4535097446409234,"d":"0.45"},{"v":0.4535097446409234,"d":"0.45"},{"v":0.272701799,"d":"0.27"}]
["38051","McIntosh","ND",{"v":0.506386846243964,"d":"0.51"},{"v":0.506386846243964,"d":"0.51"},{"v":0.219044331,"d":"0.22"}]
["38053","Mckenzie","ND",{"v":0.5350208015467264,"d":"0.54"},{"v":0.5350208015467264,"d":"0.54"},{"v":0.18657222,"d":"0.19"}]
["38055","Mclean","ND",{"v":0.5211663922523999,"d":"0.52"},{"v":0.5211663922523999,"d":"0.52"},{"v":0.171181603,"d":"0.17"}]
["38057","Mercer","ND",{"v":0.537586086693713,"d":"0.54"},{"v":0.5375860866937129,"d":"0.54"},{"v":0.205003594,"d":"0.21"}]
["38059","Morton","ND",{"v":0.3876428238371696,"d":"0.39"},{"v":0.38764282383716947,"d":"0.39"},{"v":0.11406306099999998,"d":"0.11"}]
["38061","Mountrail","ND",{"v":0.5325381334286698,"d":"0.53"},{"v":0.5325381334286698,"d":"0.53"},{"v":0.237936715,"d":"0.24"}]
["38063","Nelson","ND",{"v":0.48734319543145055,"d":"0.49"},{"v":0.48734319543145055,"d":"0.49"},{"v":0.280937924,"d":"0.28"}]
["38065","Oliver","ND",{"v":0.5647899057611369,"d":"0.56"},{"v":0.5647899057611369,"d":"0.56"},{"v":0.22466581299999996,"d":"0.22"}]
["38067","Pembina","ND",{"v":0.5235625534644688,"d":"0.52"},{"v":0.5235625534644688,"d":"0.52"},{"v":0.24391626399999997,"d":"0.24"}]
["38069","Pierce","ND",{"v":0.5656813749866604,"d":"0.57"},{"v":0.5656813749866604,"d":"0.57"},{"v":0.217771004,"d":"0.22"}]
["38071","Ramsey","ND",{"v":0.5290994836489115,"d":"0.53"},{"v":0.5290994836489115,"d":"0.53"},{"v":0.16194245,"d":"0.16"}]
["38073","Ransom","ND",{"v":0.541862504647271,"d":"0.54"},{"v":0.541862504647271,"d":"0.54"},{"v":0.227434081,"d":"0.23"}]
["38075","Renville","ND",{"v":0.5740734894888206,"d":"0.57"},{"v":0.5740734894888206,"d":"0.57"},{"v":0.268066091,"d":"0.27"}]
["38077","Richland","ND",{"v":0.5162234812291542,"d":"0.52"},{"v":0.5162234812291542,"d":"0.52"},{"v":0.168260086,"d":"0.17"}]
["38079","Rolette","ND",{"v":0.5819450401207503,"d":"0.58"},{"v":0.5819450401207504,"d":"0.58"},{"v":0.301986716,"d":"0.30"}]
["38081","Sargent","ND",{"v":0.5646602674601535,"d":"0.56"},{"v":0.5646602674601535,"d":"0.56"},{"v":0.226500152,"d":"0.23"}]
["38083","Sheridan","ND",{"v":0.4920687177838113,"d":"0.49"},{"v":0.49206871778381134,"d":"0.49"},{"v":0.251279956,"d":"0.25"}]
["38085","Sioux","ND",{"v":0.3978539926050659,"d":"0.40"},{"v":0.3978539926050658,"d":"0.40"},{"v":0.21783563,"d":"0.22"}]
["38087","Slope","ND",{"v":0.5599750056735648,"d":"0.56"},{"v":0.5599750056735647,"d":"0.56"},{"v":0.185314868,"d":"0.19"}]
["38089","Stark","ND",{"v":0.46681788547805547,"d":"0.47"},{"v":0.46681788547805547,"d":"0.47"},{"v":0.116446766,"d":"0.12"}]
["38091","Steele","ND",{"v":0.5424371987349876,"d":"0.54"},{"v":0.5424371987349876,"d":"0.54"},{"v":0.246380761,"d":"0.25"}]
["38093","Stutsman","ND",{"v":0.515785518894686,"d":"0.52"},{"v":0.515785518894686,"d":"0.52"},{"v":0.134743441,"d":"0.13"}]
["38095","Towner","ND",{"v":0.577030470893108,"d":"0.58"},{"v":0.577030470893108,"d":"0.58"},{"v":0.276304321,"d":"0.28"}]
["38097","Traill","ND",{"v":0.49075626858974336,"d":"0.49"},{"v":0.4907562685897433,"d":"0.49"},{"v":0.248987342,"d":"0.25"}]
["38099","Walsh","ND",{"v":0.5319258759734898,"d":"0.53"},{"v":0.5319258759734898,"d":"0.53"},{"v":0.20643160700000002,"d":"0.21"}]
["38101","Ward","ND",{"v":0.5037233421032609,"d":"0.50"},{"v":0.503723342103261,"d":"0.50"},{"v":0.138554767,"d":"0.14"}]
["38103","Wells","ND",{"v":0.5709879579207386,"d":"0.57"},{"v":0.5709879579207386,"d":"0.57"},{"v":0.251881633,"d":"0.25"}]
["38105","Williams","ND",{"v":0.5515423798067923,"d":"0.55"},{"v":0.5515423798067923,"d":"0.55"},{"v":0.152277263,"d":"0.15"}]
["39001","Adams","OH",{"v":3.3566588442141616,"d":"3.36"},{"v":3.3566588442141616,"d":"3.36"},{"v":0.807874602,"d":"0.81"}]
["39003","Allen","OH",{"v":2.9795480218117487,"d":"2.98"},{"v":2.9795480218117483,"d":"2.98"},{"v":0.379057144,"d":"0.38"}]
["39005","Ashland","OH",{"v":3.0474207914281872,"d":"3.05"},{"v":3.047420791428187,"d":"3.05"},{"v":0.567414498,"d":"0.57"}]
["39007","Ashtabula","OH",{"v":3.039007615775224,"d":"3.04"},{"v":3.039007615775224,"d":"3.04"},{"v":0.56580169,"d":"0.57"}]
["39009","Athens","OH",{"v":3.080673086397186,"d":"3.08"},{"v":3.080673086397186,"d":"3.08"},{"v":0.794330801,"d":"0.79"}]
["39011","Auglaize","OH",{"v":3.0481883527810605,"d":"3.05"},{"v":3.0481883527810605,"d":"3.05"},{"v":0.380247821,"d":"0.38"}]
["39013","Belmont","OH",{"v":2.9350412315679755,"d":"2.94"},{"v":2.935041231567976,"d":"2.94"},{"v":0.610785295,"d":"0.61"}]
["39015","Brown","OH",{"v":3.298105590929216,"d":"3.30"},{"v":3.2981055909292163,"d":"3.30"},{"v":0.627389433,"d":"0.63"}]
["39017","Butler","OH",{"v":2.717578950182156,"d":"2.72"},{"v":2.717578950182156,"d":"2.72"},{"v":0.455059908,"d":"0.46"}]
["39019","Carroll","OH",{"v":3.1244671343907253,"d":"3.12"},{"v":3.1244671343907253,"d":"3.12"},{"v":0.777691242,"d":"0.78"}]
["39021","Champaign","OH",{"v":3.211069497045301,"d":"3.21"},{"v":3.211069497045301,"d":"3.21"},{"v":0.48877150500000005,"d":"0.49"}]
["39023","Clark","OH",{"v":2.9949318635042603,"d":"2.99"},{"v":2.9949318635042603,"d":"2.99"},{"v":0.36680762800000005,"d":"0.37"}]
["39025","Clermont","OH",{"v":3.1311278931517945,"d":"3.13"},{"v":3.131127893151794,"d":"3.13"},{"v":0.576468293,"d":"0.58"}]
["39027","Clinton","OH",{"v":3.1459002421018067,"d":"3.15"},{"v":3.145900242101807,"d":"3.15"},{"v":0.412091659,"d":"0.41"}]
["39029","Columbiana","OH",{"v":3.049889925869029,"d":"3.05"},{"v":3.0498899258690284,"d":"3.05"},{"v":0.625642758,"d":"0.63"}]
["39031","Coshocton","OH",{"v":3.078112892310877,"d":"3.08"},{"v":3.078112892310877,"d":"3.08"},{"v":0.738337734,"d":"0.74"}]
["39033","Crawford","OH",{"v":3.0089098590308634,"d":"3.01"},{"v":3.0089098590308634,"d":"3.01"},{"v":0.374846966,"d":"0.37"}]
["39035","Cuyahoga","OH",{"v":3.198228256976578E-3,"d":"0.00"},{"v":0.003198228256976577,"d":"0.00"},{"v":1.36894757,"d":"1.37"}]
["39037","Darke","OH",{"v":3.177251014789532,"d":"3.18"},{"v":3.177251014789532,"d":"3.18"},{"v":0.444334058,"d":"0.44"}]
["39039","Defiance","OH",{"v":3.0905700189903333,"d":"3.09"},{"v":3.090570018990333,"d":"3.09"},{"v":0.414508867,"d":"0.41"}]
["39041","Delaware","OH",{"v":2.913625049056248,"d":"2.91"},{"v":2.913625049056248,"d":"2.91"},{"v":0.36743827400000006,"d":"0.37"}]
["39043","Erie","OH",{"v":2.9388958669262273,"d":"2.94"},{"v":2.9388958669262273,"d":"2.94"},{"v":0.387101471,"d":"0.39"}]
["39045","Fairfield","OH",{"v":3.040793190509722,"d":"3.04"},{"v":3.0407931905097216,"d":"3.04"},{"v":0.446021611,"d":"0.45"}]
["39047","Fayette","OH",{"v":2.940920505689943,"d":"2.94"},{"v":2.9409205056899435,"d":"2.94"},{"v":0.3659775270000001,"d":"0.37"}]
["39049","Franklin","OH",{"v":0.03890039303614506,"d":"0.04"},{"v":0.038900393036145064,"d":"0.04"},{"v":0.901518847,"d":"0.90"}]
["39051","Fulton","OH",{"v":2.9904239978330476,"d":"2.99"},{"v":2.9904239978330476,"d":"2.99"},{"v":0.41496343,"d":"0.41"}]
["39053","Gallia","OH",{"v":3.290624787723535,"d":"3.29"},{"v":3.290624787723535,"d":"3.29"},{"v":0.765298535,"d":"0.77"}]
["39055","Geauga","OH",{"v":3.084804809444694,"d":"3.08"},{"v":3.084804809444694,"d":"3.08"},{"v":0.730350419,"d":"0.73"}]
["39057","Greene","OH",{"v":2.9504444352054806,"d":"2.95"},{"v":2.9504444352054806,"d":"2.95"},{"v":0.340613056,"d":"0.34"}]
["39059","Guernsey","OH",{"v":3.0121118857499747,"d":"3.01"},{"v":3.0121118857499742,"d":"3.01"},{"v":0.661579832,"d":"0.66"}]
["39061","Hamilton","OH",{"v":0.1010038823174047,"d":"0.10"},{"v":0.10100388231740472,"d":"0.10"},{"v":0.967979371,"d":"0.97"}]
["39063","Hancock","OH",{"v":2.9765285577265397,"d":"2.98"},{"v":2.9765285577265392,"d":"2.98"},{"v":0.348563786,"d":"0.35"}]
["39065","Hardin","OH",{"v":3.0671613245064453,"d":"3.07"},{"v":3.0671613245064457,"d":"3.07"},{"v":0.41254776600000004,"d":"0.41"}]
["39067","Harrison","OH",{"v":3.188162745348782,"d":"3.19"},{"v":3.1881627453487824,"d":"3.19"},{"v":0.815268568,"d":"0.82"}]
["39069","Henry","OH",{"v":3.2216711683554395,"d":"3.22"},{"v":3.2216711683554395,"d":"3.22"},{"v":0.412591273,"d":"0.41"}]
["39071","Highland","OH",{"v":3.2173222276880638,"d":"3.22"},{"v":3.217322227688064,"d":"3.22"},{"v":0.544796948,"d":"0.54"}]
["39073","Hocking","OH",{"v":3.190552072818115,"d":"3.19"},{"v":3.190552072818115,"d":"3.19"},{"v":0.955390196,"d":"0.96"}]
["39075","Holmes","OH",{"v":3.0395061181075387,"d":"3.04"},{"v":3.0395061181075382,"d":"3.04"},{"v":0.669720623,"d":"0.67"}]
["39077","Huron","OH",{"v":3.024423023623537,"d":"3.02"},{"v":3.0244230236235374,"d":"3.02"},{"v":0.486062737,"d":"0.49"}]
["39079","Jackson","OH",{"v":3.1864816233441315,"d":"3.19"},{"v":3.1864816233441315,"d":"3.19"},{"v":0.700388471,"d":"0.70"}]
["39081","Jefferson","OH",{"v":2.9928086363472164,"d":"2.99"},{"v":2.9928086363472164,"d":"2.99"},{"v":0.71741917,"d":"0.72"}]
["39083","Knox","OH",{"v":3.0852398545234045,"d":"3.09"},{"v":3.085239854523405,"d":"3.09"},{"v":0.5714635,"d":"0.57"}]
["39085","Lake","OH",{"v":2.058540848274696,"d":"2.06"},{"v":2.058540848274696,"d":"2.06"},{"v":0.545065299,"d":"0.55"}]
["39087","Lawrence","OH",{"v":3.1736982943838377,"d":"3.17"},{"v":3.1736982943838377,"d":"3.17"},{"v":0.736994164,"d":"0.74"}]
["39089","Licking","OH",{"v":3.047532461206441,"d":"3.05"},{"v":3.047532461206441,"d":"3.05"},{"v":0.464780637,"d":"0.46"}]
["39091","Logan","OH",{"v":3.1039438653428353,"d":"3.10"},{"v":3.1039438653428353,"d":"3.10"},{"v":0.46484310000000006,"d":"0.46"}]
["39093","Lorain","OH",{"v":2.7733888270722846,"d":"2.77"},{"v":2.7733888270722846,"d":"2.77"},{"v":0.452000215,"d":"0.45"}]
["39095","Lucas","OH",{"v":1.279548822550096,"d":"1.28"},{"v":1.279548822550096,"d":"1.28"},{"v":0.551146685,"d":"0.55"}]
["39097","Madison","OH",{"v":3.1073848447235144,"d":"3.11"},{"v":3.107384844723515,"d":"3.11"},{"v":0.358427192,"d":"0.36"}]
["39099","Mahoning","OH",{"v":2.726524704730161,"d":"2.73"},{"v":2.7265247047301604,"d":"2.73"},{"v":0.478526164,"d":"0.48"}]
["39101","Marion","OH",{"v":2.939476482092203,"d":"2.94"},{"v":2.9394764820922026,"d":"2.94"},{"v":0.325548546,"d":"0.33"}]
["39103","Medina","OH",{"v":2.938508511415487,"d":"2.94"},{"v":2.938508511415487,"d":"2.94"},{"v":0.519006954,"d":"0.52"}]
["39105","Meigs","OH",{"v":3.1912914147903595,"d":"3.19"},{"v":3.1912914147903595,"d":"3.19"},{"v":0.7904722710000001,"d":"0.79"}]
["39107","Mercer","OH",{"v":3.0665596705839984,"d":"3.07"},{"v":3.066559670583999,"d":"3.07"},{"v":0.404072346,"d":"0.40"}]
["39109","Miami","OH",{"v":3.0819912156785296,"d":"3.08"},{"v":3.0819912156785296,"d":"3.08"},{"v":0.386349488,"d":"0.39"}]
["39111","Monroe","OH",{"v":2.9735342803069513,"d":"2.97"},{"v":2.9735342803069513,"d":"2.97"},{"v":0.782785322,"d":"0.78"}]
["39113","Montgomery","OH",{"v":1.5349793483840233,"d":"1.53"},{"v":1.5349793483840233,"d":"1.53"},{"v":0.474224238,"d":"0.47"}]
["39115","Morgan","OH",{"v":3.1772149032730064,"d":"3.18"},{"v":3.177214903273007,"d":"3.18"},{"v":0.784267424,"d":"0.78"}]
["39117","Morrow","OH",{"v":3.21328559672302,"d":"3.21"},{"v":3.2132855967230203,"d":"3.21"},{"v":0.60831592,"d":"0.61"}]
["39119","Muskingum","OH",{"v":2.906782511654253,"d":"2.91"},{"v":2.9067825116542525,"d":"2.91"},{"v":0.55201314,"d":"0.55"}]
["39121","Noble","OH",{"v":3.010266604324195,"d":"3.01"},{"v":3.0102666043241952,"d":"3.01"},{"v":0.707278784,"d":"0.71"}]
["39123","Ottawa","OH",{"v":3.055716827703866,"d":"3.06"},{"v":3.0557168277038667,"d":"3.06"},{"v":0.381864491,"d":"0.38"}]
["39125","Paulding","OH",{"v":3.218237094528795,"d":"3.22"},{"v":3.2182370945287953,"d":"3.22"},{"v":0.48777721799999996,"d":"0.49"}]
["39127","Perry","OH",{"v":3.122385930358749,"d":"3.12"},{"v":3.122385930358749,"d":"3.12"},{"v":0.6913816,"d":"0.69"}]
["39129","Pickaway","OH",{"v":3.1165236152239837,"d":"3.12"},{"v":3.116523615223984,"d":"3.12"},{"v":0.385783013,"d":"0.39"}]
["39131","Pike","OH",{"v":3.2941467181144493,"d":"3.29"},{"v":3.2941467181144497,"d":"3.29"},{"v":0.772276931,"d":"0.77"}]
["39133","Portage","OH",{"v":3.0284856083284346,"d":"3.03"},{"v":3.028485608328434,"d":"3.03"},{"v":0.586754388,"d":"0.59"}]
["39135","Preble","OH",{"v":3.1560644032017744,"d":"3.16"},{"v":3.156064403201775,"d":"3.16"},{"v":0.449838645,"d":"0.45"}]
["39137","Putnam","OH",{"v":3.095702361368513,"d":"3.10"},{"v":3.0957023613685126,"d":"3.10"},{"v":0.49452766,"d":"0.49"}]
["39139","Richland","OH",{"v":2.95343816252573,"d":"2.95"},{"v":2.95343816252573,"d":"2.95"},{"v":0.496376058,"d":"0.50"}]
["39141","Ross","OH",{"v":3.1655834763823263,"d":"3.17"},{"v":3.1655834763823263,"d":"3.17"},{"v":0.582035718,"d":"0.58"}]
["39143","Sandusky","OH",{"v":3.0013627802581033,"d":"3.00"},{"v":3.001362780258103,"d":"3.00"},{"v":0.381254307,"d":"0.38"}]
["39145","Scioto","OH",{"v":3.1636854760693494,"d":"3.16"},{"v":3.1636854760693494,"d":"3.16"},{"v":0.711237416,"d":"0.71"}]
["39147","Seneca","OH",{"v":3.048524300736556,"d":"3.05"},{"v":3.0485243007365557,"d":"3.05"},{"v":0.407631837,"d":"0.41"}]
["39149","Shelby","OH",{"v":2.9465715341088936,"d":"2.95"},{"v":2.9465715341088936,"d":"2.95"},{"v":0.42919789700000005,"d":"0.43"}]
["39151","Stark","OH",{"v":2.6265759528227073,"d":"2.63"},{"v":2.6265759528227073,"d":"2.63"},{"v":0.457995141,"d":"0.46"}]
["39153","Summit","OH",{"v":1.1562281767244589,"d":"1.16"},{"v":1.1562281767244587,"d":"1.16"},{"v":0.691097783,"d":"0.69"}]
["39155","Trumbull","OH",{"v":2.882772141102961,"d":"2.88"},{"v":2.882772141102961,"d":"2.88"},{"v":0.50762017,"d":"0.51"}]
["39157","Tuscarawas","OH",{"v":2.9040914801509783,"d":"2.90"},{"v":2.9040914801509783,"d":"2.90"},{"v":0.581749336,"d":"0.58"}]
["39159","Union","OH",{"v":3.03870523663789,"d":"3.04"},{"v":3.0387052366378895,"d":"3.04"},{"v":0.384123921,"d":"0.38"}]
["39161","Van Wert","OH",{"v":3.020257390765901,"d":"3.02"},{"v":3.0202573907659014,"d":"3.02"},{"v":0.390580401,"d":"0.39"}]
["39163","Vinton","OH",{"v":3.354729544665079,"d":"3.35"},{"v":3.354729544665079,"d":"3.35"},{"v":1.094012402,"d":"1.09"}]
["39165","Warren","OH",{"v":2.9564262314400565,"d":"2.96"},{"v":2.9564262314400565,"d":"2.96"},{"v":0.45625745999999995,"d":"0.46"}]
["39167","Washington","OH",{"v":2.9538492545577295,"d":"2.95"},{"v":2.953849254557729,"d":"2.95"},{"v":0.621675205,"d":"0.62"}]
["39169","Wayne","OH",{"v":2.9701350380367977,"d":"2.97"},{"v":2.970135038036798,"d":"2.97"},{"v":0.45237187400000006,"d":"0.45"}]
["39171","Williams","OH",{"v":3.057366153917622,"d":"3.06"},{"v":3.057366153917622,"d":"3.06"},{"v":0.435459947,"d":"0.44"}]
["39173","Wood","OH",{"v":2.9909737561604643,"d":"2.99"},{"v":2.990973756160464,"d":"2.99"},{"v":0.336103601,"d":"0.34"}]
["39175","Wyandot","OH",{"v":3.1059385991658064,"d":"3.11"},{"v":3.1059385991658064,"d":"3.11"},{"v":0.435150946,"d":"0.44"}]
["40001","Adair","OK",{"v":2.637711263073848,"d":"2.64"},{"v":2.637711263073848,"d":"2.64"},{"v":0.404589947,"d":"0.40"}]
["40003","Alfalfa","OK",{"v":2.303486445210043,"d":"2.30"},{"v":2.303486445210043,"d":"2.30"},{"v":0.220412512,"d":"0.22"}]
["40005","Atoka","OK",{"v":2.4980727373950833,"d":"2.50"},{"v":2.498072737395083,"d":"2.50"},{"v":0.384555822,"d":"0.38"}]
["40007","Beaver","OK",{"v":2.3459874447893814,"d":"2.35"},{"v":2.345987444789382,"d":"2.35"},{"v":0.21835903299999998,"d":"0.22"}]
["40009","Beckham","OK",{"v":2.2189644792478336,"d":"2.22"},{"v":2.2189644792478336,"d":"2.22"},{"v":0.164478289,"d":"0.16"}]
["40011","Blaine","OK",{"v":2.3006423750258977,"d":"2.30"},{"v":2.3006423750258977,"d":"2.30"},{"v":0.212677152,"d":"0.21"}]
["40013","Bryan","OK",{"v":2.4626253034078407,"d":"2.46"},{"v":2.4626253034078407,"d":"2.46"},{"v":0.251620373,"d":"0.25"}]
["40015","Caddo","OK",{"v":2.2521748549071994,"d":"2.25"},{"v":2.2521748549072,"d":"2.25"},{"v":0.203759413,"d":"0.20"}]
["40017","Canadian","OK",{"v":2.175856669401837,"d":"2.18"},{"v":2.1758566694018366,"d":"2.18"},{"v":0.150465844,"d":"0.15"}]
["40019","Carter","OK",{"v":2.252305447083362,"d":"2.25"},{"v":2.252305447083362,"d":"2.25"},{"v":0.219544778,"d":"0.22"}]
["40021","Cherokee","OK",{"v":2.554403888304,"d":"2.55"},{"v":2.554403888304,"d":"2.55"},{"v":0.353608295,"d":"0.35"}]
["40023","Choctaw","OK",{"v":2.527190588167064,"d":"2.53"},{"v":2.527190588167064,"d":"2.53"},{"v":0.299413995,"d":"0.30"}]
["40025","Cimarron","OK",{"v":2.308426623742578,"d":"2.31"},{"v":2.308426623742578,"d":"2.31"},{"v":0.20676687999999996,"d":"0.21"}]
["40027","Cleveland","OK",{"v":2.1220363747223243,"d":"2.12"},{"v":2.1220363747223243,"d":"2.12"},{"v":0.246711432,"d":"0.25"}]
["40029","Coal","OK",{"v":2.2472301182051257,"d":"2.25"},{"v":2.2472301182051253,"d":"2.25"},{"v":0.293114675,"d":"0.29"}]
["40031","Comanche","OK",{"v":2.1875904083322912,"d":"2.19"},{"v":2.1875904083322912,"d":"2.19"},{"v":0.153078262,"d":"0.15"}]
["40033","Cotton","OK",{"v":2.2374987519266285,"d":"2.24"},{"v":2.2374987519266285,"d":"2.24"},{"v":0.17143123599999996,"d":"0.17"}]
["40035","Craig","OK",{"v":2.3563664964399873,"d":"2.36"},{"v":2.3563664964399873,"d":"2.36"},{"v":0.24219075199999998,"d":"0.24"}]
["40037","Creek","OK",{"v":2.283300331516877,"d":"2.28"},{"v":2.283300331516877,"d":"2.28"},{"v":0.276722532,"d":"0.28"}]
["40039","Custer","OK",{"v":2.258774209876463,"d":"2.26"},{"v":2.258774209876463,"d":"2.26"},{"v":0.166893649,"d":"0.17"}]
["40041","Delaware","OK",{"v":2.742934496205863,"d":"2.74"},{"v":2.7429344962058635,"d":"2.74"},{"v":0.415562165,"d":"0.42"}]
["40043","Dewey","OK",{"v":2.3331821525003664,"d":"2.33"},{"v":2.3331821525003664,"d":"2.33"},{"v":0.258182129,"d":"0.26"}]
["40045","Ellis","OK",{"v":2.3766156999376618,"d":"2.38"},{"v":2.376615699937662,"d":"2.38"},{"v":0.250144783,"d":"0.25"}]
["40047","Garfield","OK",{"v":2.238570733558073,"d":"2.24"},{"v":2.238570733558073,"d":"2.24"},{"v":0.155335618,"d":"0.16"}]
["40049","Garvin","OK",{"v":2.2900861363871123,"d":"2.29"},{"v":2.2900861363871123,"d":"2.29"},{"v":0.23335589100000004,"d":"0.23"}]
["40051","Grady","OK",{"v":2.3046567640549878,"d":"2.30"},{"v":2.3046567640549878,"d":"2.30"},{"v":0.22786453,"d":"0.23"}]
["40053","Grant","OK",{"v":2.301025097359279,"d":"2.30"},{"v":2.3010250973592785,"d":"2.30"},{"v":0.214506135,"d":"0.21"}]
["40055","Greer","OK",{"v":2.070358089833947,"d":"2.07"},{"v":2.0703580898339466,"d":"2.07"},{"v":0.13217734,"d":"0.13"}]
["40057","Harmon","OK",{"v":2.1234587154183657,"d":"2.12"},{"v":2.1234587154183657,"d":"2.12"},{"v":0.158347871,"d":"0.16"}]
["40059","Harper","OK",{"v":2.340639692909298,"d":"2.34"},{"v":2.340639692909298,"d":"2.34"},{"v":0.226125498,"d":"0.23"}]
["40061","Haskell","OK",{"v":2.5597795959076293,"d":"2.56"},{"v":2.5597795959076293,"d":"2.56"},{"v":0.302008246,"d":"0.30"}]
["40063","Hughes","OK",{"v":2.3250218025009635,"d":"2.33"},{"v":2.3250218025009635,"d":"2.33"},{"v":0.327121301,"d":"0.33"}]
["40065","Jackson","OK",{"v":2.14879559934268,"d":"2.15"},{"v":2.14879559934268,"d":"2.15"},{"v":0.125366466,"d":"0.13"}]
["40067","Jefferson","OK",{"v":2.1633395064405714,"d":"2.16"},{"v":2.1633395064405714,"d":"2.16"},{"v":0.187588655,"d":"0.19"}]
["40069","Johnston","OK",{"v":2.3264044103912203,"d":"2.33"},{"v":2.3264044103912207,"d":"2.33"},{"v":0.316326903,"d":"0.32"}]
["40071","Kay","OK",{"v":2.207051505875059,"d":"2.21"},{"v":2.2070515058750595,"d":"2.21"},{"v":0.15039422,"d":"0.15"}]
["40073","Kingfisher","OK",{"v":2.266333023356343,"d":"2.27"},{"v":2.266333023356343,"d":"2.27"},{"v":0.184126951,"d":"0.18"}]
["40075","Kiowa","OK",{"v":2.166125018700533,"d":"2.17"},{"v":2.166125018700533,"d":"2.17"},{"v":0.155830789,"d":"0.16"}]
["40077","Latimer","OK",{"v":2.5701131234837566,"d":"2.57"},{"v":2.5701131234837566,"d":"2.57"},{"v":0.40725618,"d":"0.41"}]
["40079","Le Flore","OK",{"v":2.486463302763651,"d":"2.49"},{"v":2.486463302763651,"d":"2.49"},{"v":0.378264936,"d":"0.38"}]
["40081","Lincoln","OK",{"v":2.3561906446101326,"d":"2.36"},{"v":2.3561906446101326,"d":"2.36"},{"v":0.295805215,"d":"0.30"}]
["40083","Logan","OK",{"v":2.2915813932729314,"d":"2.29"},{"v":2.2915813932729314,"d":"2.29"},{"v":0.228314098,"d":"0.23"}]
["40085","Love","OK",{"v":2.3532171786294,"d":"2.35"},{"v":2.3532171786293996,"d":"2.35"},{"v":0.303024562,"d":"0.30"}]
["40087","Mcclain","OK",{"v":2.2977077368041736,"d":"2.30"},{"v":2.2977077368041736,"d":"2.30"},{"v":0.24329740100000002,"d":"0.24"}]
["40089","McCurtain","OK",{"v":2.5418297270483876,"d":"2.54"},{"v":2.5418297270483876,"d":"2.54"},{"v":0.420104319,"d":"0.42"}]
["40091","McIntosh","OK",{"v":2.3833490543211457,"d":"2.38"},{"v":2.383349054321146,"d":"2.38"},{"v":0.297260687,"d":"0.30"}]
["40093","Major","OK",{"v":2.3607013125822562,"d":"2.36"},{"v":2.3607013125822567,"d":"2.36"},{"v":0.259826998,"d":"0.26"}]
["40095","Marshall","OK",{"v":2.356774038847583,"d":"2.36"},{"v":2.3567740388475826,"d":"2.36"},{"v":0.26693427,"d":"0.27"}]
["40097","Mayes","OK",{"v":2.708282092338561,"d":"2.71"},{"v":2.7082820923385613,"d":"2.71"},{"v":0.331325288,"d":"0.33"}]
["40099","Murray","OK",{"v":2.28417749690479,"d":"2.28"},{"v":2.28417749690479,"d":"2.28"},{"v":0.21928016,"d":"0.22"}]
["40101","Muskogee","OK",{"v":2.2394591454367174,"d":"2.24"},{"v":2.2394591454367174,"d":"2.24"},{"v":0.214718519,"d":"0.21"}]
["40103","Noble","OK",{"v":2.3508301987853417,"d":"2.35"},{"v":2.3508301987853417,"d":"2.35"},{"v":0.219661276,"d":"0.22"}]
["40105","Nowata","OK",{"v":2.3303563794352256,"d":"2.33"},{"v":2.330356379435225,"d":"2.33"},{"v":0.229036662,"d":"0.23"}]
["40107","Okfuskee","OK",{"v":2.3248628307336694,"d":"2.32"},{"v":2.3248628307336694,"d":"2.32"},{"v":0.299468277,"d":"0.30"}]
["40109","Oklahoma","OK",{"v":1.506625405936756,"d":"1.51"},{"v":1.506625405936756,"d":"1.51"},{"v":0.267826431,"d":"0.27"}]
["40111","Okmulgee","OK",{"v":2.240460424514379,"d":"2.24"},{"v":2.240460424514379,"d":"2.24"},{"v":0.239767992,"d":"0.24"}]
["40113","Osage","OK",{"v":2.324598314297714,"d":"2.32"},{"v":2.3245983142977136,"d":"2.32"},{"v":0.2383917,"d":"0.24"}]
["40115","Ottawa","OK",{"v":2.666113243362128,"d":"2.67"},{"v":2.666113243362128,"d":"2.67"},{"v":0.238096172,"d":"0.24"}]
["40117","Pawnee","OK",{"v":2.3916461313001,"d":"2.39"},{"v":2.3916461313001,"d":"2.39"},{"v":0.293284176,"d":"0.29"}]
["40119","Payne","OK",{"v":2.208779150902127,"d":"2.21"},{"v":2.2087791509021275,"d":"2.21"},{"v":0.202572637,"d":"0.20"}]
["40121","Pittsburg","OK",{"v":2.576646293669567,"d":"2.58"},{"v":2.5766462936695675,"d":"2.58"},{"v":0.285464741,"d":"0.29"}]
["40123","Pontotoc","OK",{"v":2.1816097044009726,"d":"2.18"},{"v":2.181609704400972,"d":"2.18"},{"v":0.230201782,"d":"0.23"}]
["40125","Pottawatomie","OK",{"v":2.2379979954359444,"d":"2.24"},{"v":2.2379979954359444,"d":"2.24"},{"v":0.247349835,"d":"0.25"}]
["40127","Pushmataha","OK",{"v":2.602777631623505,"d":"2.60"},{"v":2.602777631623505,"d":"2.60"},{"v":0.49990833,"d":"0.50"}]
["40129","Roger Mills","OK",{"v":2.341286541293297,"d":"2.34"},{"v":2.341286541293297,"d":"2.34"},{"v":0.240636574,"d":"0.24"}]
["40131","Rogers","OK",{"v":2.245493982710416,"d":"2.25"},{"v":2.245493982710416,"d":"2.25"},{"v":0.22890073,"d":"0.23"}]
["40133","Seminole","OK",{"v":2.312293592918307,"d":"2.31"},{"v":2.312293592918307,"d":"2.31"},{"v":0.306655959,"d":"0.31"}]
["40135","Sequoyah","OK",{"v":2.6982231028152914,"d":"2.70"},{"v":2.698223102815292,"d":"2.70"},{"v":0.346328697,"d":"0.35"}]
["40137","Stephens","OK",{"v":2.1906781183145267,"d":"2.19"},{"v":2.1906781183145267,"d":"2.19"},{"v":0.178315721,"d":"0.18"}]
["40139","Texas","OK",{"v":2.3302487059520076,"d":"2.33"},{"v":2.3302487059520076,"d":"2.33"},{"v":0.178619708,"d":"0.18"}]
["40141","Tillman","OK",{"v":2.136888437252647,"d":"2.14"},{"v":2.1368884372526464,"d":"2.14"},{"v":0.138898445,"d":"0.14"}]
["40143","Tulsa","OK",{"v":1.4353440687339953,"d":"1.44"},{"v":1.435344068733995,"d":"1.44"},{"v":0.28907295,"d":"0.29"}]
["40145","Wagoner","OK",{"v":2.2608427988246698,"d":"2.26"},{"v":2.2608427988246693,"d":"2.26"},{"v":0.219951769,"d":"0.22"}]
["40147","Washington","OK",{"v":2.203517601022011,"d":"2.20"},{"v":2.203517601022011,"d":"2.20"},{"v":0.178639668,"d":"0.18"}]
["40149","Washita","OK",{"v":2.2734005178286414,"d":"2.27"},{"v":2.273400517828642,"d":"2.27"},{"v":0.181143458,"d":"0.18"}]
["40151","Woods","OK",{"v":2.236118220739523,"d":"2.24"},{"v":2.236118220739523,"d":"2.24"},{"v":0.166027315,"d":"0.17"}]
["40153","Woodward","OK",{"v":2.330210172742866,"d":"2.33"},{"v":2.3302101727428663,"d":"2.33"},{"v":0.198078586,"d":"0.20"}]
["41001","Baker","OR",{"v":4.661101073594069,"d":"4.66"},{"v":4.661101073594069,"d":"4.66"},{"v":1.192948667,"d":"1.19"}]
["41003","Benton","OR",{"v":4.1350726321806714,"d":"4.14"},{"v":4.1350726321806714,"d":"4.14"},{"v":0.806875514,"d":"0.81"}]
["41005","Clackamas","OR",{"v":4.128045836243287,"d":"4.13"},{"v":4.128045836243287,"d":"4.13"},{"v":0.910220086,"d":"0.91"}]
["41007","Clatsop","OR",{"v":4.587660773767088,"d":"4.59"},{"v":4.587660773767087,"d":"4.59"},{"v":0.821918534,"d":"0.82"}]
["41009","Columbia","OR",{"v":4.271705746466727,"d":"4.27"},{"v":4.271705746466727,"d":"4.27"},{"v":1.082729563,"d":"1.08"}]
["41011","Coos","OR",{"v":4.418105532212708,"d":"4.42"},{"v":4.418105532212708,"d":"4.42"},{"v":1.126495647,"d":"1.13"}]
["41013","Crook","OR",{"v":4.638263532038224,"d":"4.64"},{"v":4.638263532038224,"d":"4.64"},{"v":1.181018497,"d":"1.18"}]
["41015","Curry","OR",{"v":4.561553130357102,"d":"4.56"},{"v":4.561553130357101,"d":"4.56"},{"v":1.182809189,"d":"1.18"}]
["41017","Deschutes","OR",{"v":4.553689602454583,"d":"4.55"},{"v":4.553689602454583,"d":"4.55"},{"v":1.150301246,"d":"1.15"}]
["41019","Douglas","OR",{"v":4.48095921765963,"d":"4.48"},{"v":4.480959217659631,"d":"4.48"},{"v":1.27418112,"d":"1.27"}]
["41021","Gilliam","OR",{"v":4.461400837160574,"d":"4.46"},{"v":4.461400837160573,"d":"4.46"},{"v":0.920609017,"d":"0.92"}]
["41023","Grant","OR",{"v":4.877144356463857,"d":"4.88"},{"v":4.877144356463857,"d":"4.88"},{"v":2.119304261,"d":"2.12"}]
["41025","Harney","OR",{"v":4.626561968018582,"d":"4.63"},{"v":4.626561968018582,"d":"4.63"},{"v":1.173725057,"d":"1.17"}]
["41027","Hood River","OR",{"v":4.438390936199706,"d":"4.44"},{"v":4.438390936199705,"d":"4.44"},{"v":1.48085157,"d":"1.48"}]
["41029","Jackson","OR",{"v":4.315388980183639,"d":"4.32"},{"v":4.315388980183639,"d":"4.32"},{"v":1.001101717,"d":"1.00"}]
["41031","Jefferson","OR",{"v":4.7307382427435325,"d":"4.73"},{"v":4.7307382427435325,"d":"4.73"},{"v":1.450739339,"d":"1.45"}]
["41033","Josephine","OR",{"v":4.489206540145975,"d":"4.49"},{"v":4.489206540145975,"d":"4.49"},{"v":1.373342584,"d":"1.37"}]
["41035","Klamath","OR",{"v":4.703468571616076,"d":"4.70"},{"v":4.703468571616075,"d":"4.70"},{"v":1.328585875,"d":"1.33"}]
["41037","Lake","OR",{"v":4.691607630172724,"d":"4.69"},{"v":4.691607630172724,"d":"4.69"},{"v":1.407401876,"d":"1.41"}]
["41039","Lane","OR",{"v":4.339486902770592,"d":"4.34"},{"v":4.3394869027705925,"d":"4.34"},{"v":1.037055766,"d":"1.04"}]
["41041","Lincoln","OR",{"v":4.348271190050545,"d":"4.35"},{"v":4.348271190050545,"d":"4.35"},{"v":0.987669721,"d":"0.99"}]
["41043","Linn","OR",{"v":4.195046992271081,"d":"4.20"},{"v":4.195046992271081,"d":"4.20"},{"v":0.857814499,"d":"0.86"}]
["41045","Malheur","OR",{"v":4.416316870901575,"d":"4.42"},{"v":4.416316870901576,"d":"4.42"},{"v":0.793022383,"d":"0.79"}]
["41047","Marion","OR",{"v":4.041486724244121,"d":"4.04"},{"v":4.0414867242441215,"d":"4.04"},{"v":0.7613515719999999,"d":"0.76"}]
["41049","Morrow","OR",{"v":4.436749394660587,"d":"4.44"},{"v":4.436749394660587,"d":"4.44"},{"v":0.849102678,"d":"0.85"}]
["41051","Multnomah","OR",{"v":0.33404291382407947,"d":"0.33"},{"v":0.33404291382407947,"d":"0.33"},{"v":1.548075651,"d":"1.55"}]
["41053","Polk","OR",{"v":4.229530967587535,"d":"4.23"},{"v":4.229530967587534,"d":"4.23"},{"v":0.778228091,"d":"0.78"}]
["41055","Sherman","OR",{"v":4.509801434482335,"d":"4.51"},{"v":4.509801434482335,"d":"4.51"},{"v":0.929479146,"d":"0.93"}]
["41057","Tillamook","OR",{"v":4.409095407488439,"d":"4.41"},{"v":4.409095407488439,"d":"4.41"},{"v":1.2623475699999998,"d":"1.26"}]
["41059","Umatilla","OR",{"v":4.292807085428345,"d":"4.29"},{"v":4.292807085428346,"d":"4.29"},{"v":0.7026416049999998,"d":"0.70"}]
["41061","Union","OR",{"v":4.651983876383556,"d":"4.65"},{"v":4.651983876383556,"d":"4.65"},{"v":1.373992117,"d":"1.37"}]
["41063","Wallowa","OR",{"v":4.87375734501631,"d":"4.87"},{"v":4.87375734501631,"d":"4.87"},{"v":2.0229862,"d":"2.02"}]
["41065","Wasco","OR",{"v":4.404816342831078,"d":"4.40"},{"v":4.404816342831077,"d":"4.40"},{"v":0.867417942,"d":"0.87"}]
["41067","Washington","OR",{"v":3.6495851136683646,"d":"3.65"},{"v":3.649585113668365,"d":"3.65"},{"v":0.917285998,"d":"0.92"}]
["41069","Wheeler","OR",{"v":4.82144160194575,"d":"4.82"},{"v":4.82144160194575,"d":"4.82"},{"v":1.623375711,"d":"1.62"}]
["41071","Yamhill","OR",{"v":4.269768257570047,"d":"4.27"},{"v":4.269768257570046,"d":"4.27"},{"v":0.899949838,"d":"0.90"}]
["42001","Adams","PA",{"v":2.7764724710967483,"d":"2.78"},{"v":2.7764724710967483,"d":"2.78"},{"v":0.521650066,"d":"0.52"}]
["42003","Allegheny","PA",{"v":0.2075152028154198,"d":"0.21"},{"v":0.2075152028154198,"d":"0.21"},{"v":0.8213057529999999,"d":"0.82"}]
["42005","Armstrong","PA",{"v":2.4375870075012136,"d":"2.44"},{"v":2.4375870075012136,"d":"2.44"},{"v":0.579870908,"d":"0.58"}]
["42007","Beaver","PA",{"v":2.393727431857598,"d":"2.39"},{"v":2.393727431857598,"d":"2.39"},{"v":0.547118954,"d":"0.55"}]
["42009","Bedford","PA",{"v":2.948034439810815,"d":"2.95"},{"v":2.948034439810815,"d":"2.95"},{"v":1.109144214,"d":"1.11"}]
["42011","Berks","PA",{"v":2.709000352642624,"d":"2.71"},{"v":2.709000352642624,"d":"2.71"},{"v":0.47887969500000005,"d":"0.48"}]
["42013","Blair","PA",{"v":2.661520127060574,"d":"2.66"},{"v":2.6615201270605744,"d":"2.66"},{"v":0.655782106,"d":"0.66"}]
["42015","Bradford","PA",{"v":2.786957022778914,"d":"2.79"},{"v":2.7869570227789144,"d":"2.79"},{"v":0.926140233,"d":"0.93"}]
["42017","Bucks","PA",{"v":2.049418558473427,"d":"2.05"},{"v":2.049418558473427,"d":"2.05"},{"v":0.572571748,"d":"0.57"}]
["42019","Butler","PA",{"v":2.4884341979956988,"d":"2.49"},{"v":2.4884341979956988,"d":"2.49"},{"v":0.547880992,"d":"0.55"}]
["42021","Cambria","PA",{"v":2.7437491278928703,"d":"2.74"},{"v":2.7437491278928703,"d":"2.74"},{"v":0.73484034,"d":"0.73"}]
["42023","Cameron","PA",{"v":2.717188940742405,"d":"2.72"},{"v":2.717188940742405,"d":"2.72"},{"v":0.983682518,"d":"0.98"}]
["42025","Carbon","PA",{"v":2.737898442640117,"d":"2.74"},{"v":2.7378984426401165,"d":"2.74"},{"v":1.095849569,"d":"1.10"}]
["42027","Centre","PA",{"v":2.9426263754777295,"d":"2.94"},{"v":2.942626375477729,"d":"2.94"},{"v":1.071119514,"d":"1.07"}]
["42029","Chester","PA",{"v":2.573652223813687,"d":"2.57"},{"v":2.573652223813687,"d":"2.57"},{"v":0.476830462,"d":"0.48"}]
["42031","Clarion","PA",{"v":2.7114275527228147,"d":"2.71"},{"v":2.7114275527228147,"d":"2.71"},{"v":0.713210275,"d":"0.71"}]
["42033","Clearfield","PA",{"v":2.8460215961536197,"d":"2.85"},{"v":2.8460215961536197,"d":"2.85"},{"v":1.017499271,"d":"1.02"}]
["42035","Clinton","PA",{"v":2.866785054996463,"d":"2.87"},{"v":2.866785054996463,"d":"2.87"},{"v":1.287171505,"d":"1.29"}]
["42037","Columbia","PA",{"v":2.6766267997721385,"d":"2.68"},{"v":2.6766267997721385,"d":"2.68"},{"v":0.756963993,"d":"0.76"}]
["42039","Crawford","PA",{"v":2.6403344586240536,"d":"2.64"},{"v":2.6403344586240536,"d":"2.64"},{"v":0.745644896,"d":"0.75"}]
["42041","Cumberland","PA",{"v":2.736134541108449,"d":"2.74"},{"v":2.7361345411084486,"d":"2.74"},{"v":0.521207235,"d":"0.52"}]
["42043","Dauphin","PA",{"v":2.7946403368379067,"d":"2.79"},{"v":2.794640336837907,"d":"2.79"},{"v":0.664635731,"d":"0.66"}]
["42045","Delaware","PA",{"v":5.4645548466204065E-3,"d":"0.01"},{"v":5.4645548466204065E-3,"d":"0.01"},{"v":1.393806619,"d":"1.39"}]
["42047","Elk","PA",{"v":2.5354281035195094,"d":"2.54"},{"v":2.5354281035195094,"d":"2.54"},{"v":0.814353099,"d":"0.81"}]
["42049","Erie","PA",{"v":2.3674456429854915,"d":"2.37"},{"v":2.3674456429854915,"d":"2.37"},{"v":0.473308668,"d":"0.47"}]
["42051","Fayette","PA",{"v":2.766020675471028,"d":"2.77"},{"v":2.7660206754710277,"d":"2.77"},{"v":0.763818755,"d":"0.76"}]
["42053","Forest","PA",{"v":2.722546849726653,"d":"2.72"},{"v":2.7225468497266534,"d":"2.72"},{"v":1.150655586,"d":"1.15"}]
["42055","Franklin","PA",{"v":2.8058419379827493,"d":"2.81"},{"v":2.8058419379827493,"d":"2.81"},{"v":0.559560755,"d":"0.56"}]
["42057","Fulton","PA",{"v":3.006846662945681,"d":"3.01"},{"v":3.006846662945681,"d":"3.01"},{"v":1.213594521,"d":"1.21"}]
["42059","Greene","PA",{"v":2.6222620018353466,"d":"2.62"},{"v":2.622262001835347,"d":"2.62"},{"v":0.72420927,"d":"0.72"}]
["42061","Huntingdon","PA",{"v":3.0093069330685975,"d":"3.01"},{"v":3.009306933068598,"d":"3.01"},{"v":1.14005804,"d":"1.14"}]
["42063","Indiana","PA",{"v":2.538997151685019,"d":"2.54"},{"v":2.538997151685019,"d":"2.54"},{"v":0.694458911,"d":"0.69"}]
["42065","Jefferson","PA",{"v":2.6815706744109753,"d":"2.68"},{"v":2.6815706744109757,"d":"2.68"},{"v":0.7379644810000001,"d":"0.74"}]
["42067","Juniata","PA",{"v":3.0495704261357433,"d":"3.05"},{"v":3.0495704261357424,"d":"3.05"},{"v":1.097169811,"d":"1.10"}]
["42069","Lackawanna","PA",{"v":2.43734483611143,"d":"2.44"},{"v":2.4373448361114303,"d":"2.44"},{"v":0.763929187,"d":"0.76"}]
["42071","Lancaster","PA",{"v":2.632608881979751,"d":"2.63"},{"v":2.6326088819797504,"d":"2.63"},{"v":0.421326192,"d":"0.42"}]
["42073","Lawrence","PA",{"v":2.46425265871581,"d":"2.46"},{"v":2.4642526587158105,"d":"2.46"},{"v":0.510138812,"d":"0.51"}]
["42075","Lebanon","PA",{"v":2.752281348083828,"d":"2.75"},{"v":2.752281348083828,"d":"2.75"},{"v":0.486855677,"d":"0.49"}]
["42077","Lehigh","PA",{"v":2.10401191611547,"d":"2.10"},{"v":2.10401191611547,"d":"2.10"},{"v":0.711256223,"d":"0.71"}]
["42079","Luzerne","PA",{"v":2.689363208944406,"d":"2.69"},{"v":2.689363208944406,"d":"2.69"},{"v":0.9086373330000002,"d":"0.91"}]
["42081","Lycoming","PA",{"v":2.750253585317579,"d":"2.75"},{"v":2.7502535853175796,"d":"2.75"},{"v":0.801163561,"d":"0.80"}]
["42083","McKean","PA",{"v":2.462382507414128,"d":"2.46"},{"v":2.462382507414128,"d":"2.46"},{"v":0.757879759,"d":"0.76"}]
["42085","Mercer","PA",{"v":2.575324343322179,"d":"2.58"},{"v":2.575324343322179,"d":"2.58"},{"v":0.617570136,"d":"0.62"}]
["42087","Mifflin","PA",{"v":2.945169923577618,"d":"2.95"},{"v":2.945169923577618,"d":"2.95"},{"v":0.970504724,"d":"0.97"}]
["42089","Monroe","PA",{"v":2.846767802267309,"d":"2.85"},{"v":2.846767802267309,"d":"2.85"},{"v":1.395529295,"d":"1.40"}]
["42091","Montgomery","PA",{"v":0.49585371006236667,"d":"0.50"},{"v":0.4958537100623666,"d":"0.50"},{"v":0.676424726,"d":"0.68"}]
["42093","Montour","PA",{"v":2.7834704962480483,"d":"2.78"},{"v":2.7834704962480483,"d":"2.78"},{"v":0.623480931,"d":"0.62"}]
["42095","Northampton","PA",{"v":2.500156242790795,"d":"2.50"},{"v":2.5001562427907955,"d":"2.50"},{"v":0.682424651,"d":"0.68"}]
["42097","Northumberland","PA",{"v":2.852533666236341,"d":"2.85"},{"v":2.8525336662363414,"d":"2.85"},{"v":0.677561145,"d":"0.68"}]
["42099","Perry","PA",{"v":3.044945151718499,"d":"3.04"},{"v":3.044945151718499,"d":"3.04"},{"v":1.109988383,"d":"1.11"}]
["42101","Philadelphia","PA",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["42103","Pike","PA",{"v":2.8881790234697324,"d":"2.89"},{"v":2.888179023469732,"d":"2.89"},{"v":1.47532836,"d":"1.48"}]
["42105","Potter","PA",{"v":2.542476993814939,"d":"2.54"},{"v":2.5424769938149385,"d":"2.54"},{"v":0.939593233,"d":"0.94"}]
["42107","Schuylkill","PA",{"v":2.918039764982071,"d":"2.92"},{"v":2.9180397649820704,"d":"2.92"},{"v":1.000910194,"d":"1.00"}]
["42109","Snyder","PA",{"v":2.9334289202315587,"d":"2.93"},{"v":2.9334289202315587,"d":"2.93"},{"v":0.866592719,"d":"0.87"}]
["42111","Somerset","PA",{"v":2.8772299337719622,"d":"2.88"},{"v":2.8772299337719627,"d":"2.88"},{"v":0.907363129,"d":"0.91"}]
["42113","Sullivan","PA",{"v":2.9338940956580326,"d":"2.93"},{"v":2.933894095658033,"d":"2.93"},{"v":1.621561662,"d":"1.62"}]
["42115","Susquehanna","PA",{"v":2.836379384204564,"d":"2.84"},{"v":2.8363793842045646,"d":"2.84"},{"v":1.282013796,"d":"1.28"}]
["42117","Tioga","PA",{"v":2.653539187080626,"d":"2.65"},{"v":2.653539187080626,"d":"2.65"},{"v":0.901569579,"d":"0.90"}]
["42119","Union","PA",{"v":2.9402486340996994,"d":"2.94"},{"v":2.9402486340997,"d":"2.94"},{"v":0.881693647,"d":"0.88"}]
["42121","Venango","PA",{"v":2.709058733158012,"d":"2.71"},{"v":2.709058733158012,"d":"2.71"},{"v":0.788969401,"d":"0.79"}]
["42123","Warren","PA",{"v":2.5488735559732323,"d":"2.55"},{"v":2.5488735559732323,"d":"2.55"},{"v":0.812675128,"d":"0.81"}]
["42125","Washington","PA",{"v":2.4616249159130237,"d":"2.46"},{"v":2.461624915913024,"d":"2.46"},{"v":0.495855852,"d":"0.50"}]
["42127","Wayne","PA",{"v":2.8144038622570937,"d":"2.81"},{"v":2.8144038622570937,"d":"2.81"},{"v":1.266232426,"d":"1.27"}]
["42129","Westmoreland","PA",{"v":2.4281459153754854,"d":"2.43"},{"v":2.4281459153754854,"d":"2.43"},{"v":0.604341094,"d":"0.60"}]
["42131","Wyoming","PA",{"v":2.881733060367008,"d":"2.88"},{"v":2.8817330603670075,"d":"2.88"},{"v":1.370717368,"d":"1.37"}]
["42133","York","PA",{"v":2.662311241420856,"d":"2.66"},{"v":2.6623112414208565,"d":"2.66"},{"v":0.427557189,"d":"0.43"}]
["44001","Bristol","RI",{"v":0.10232259979354971,"d":"0.10"},{"v":0.10232259979354974,"d":"0.10"},{"v":0.839491405,"d":"0.84"}]
["44003","Kent","RI",{"v":2.0669463183704466,"d":"2.07"},{"v":2.0669463183704466,"d":"2.07"},{"v":0.755436302,"d":"0.76"}]
["44005","Newport","RI",{"v":1.505664376305353,"d":"1.51"},{"v":1.5056643763053534,"d":"1.51"},{"v":0.461659929,"d":"0.46"}]
["44007","Providence","RI",{"v":0.7862131563699201,"d":"0.79"},{"v":0.7862131563699202,"d":"0.79"},{"v":0.936548188,"d":"0.94"}]
["44009","Washington","RI",{"v":2.905996617979831,"d":"2.91"},{"v":2.905996617979831,"d":"2.91"},{"v":0.531971986,"d":"0.53"}]
["45001","Abbeville","SC",{"v":1.0053536221322985,"d":"1.01"},{"v":1.0053536221322985,"d":"1.01"},{"v":0.155087806,"d":"0.16"}]
["45003","Aiken","SC",{"v":0.9965104531381849,"d":"1.00"},{"v":0.9965104531381848,"d":"1.00"},{"v":0.122670082,"d":"0.12"}]
["45005","Allendale","SC",{"v":1.050340899882837,"d":"1.05"},{"v":1.050340899882837,"d":"1.05"},{"v":0.132883319,"d":"0.13"}]
["45007","Anderson","SC",{"v":1.0828567994683542,"d":"1.08"},{"v":1.082856799468354,"d":"1.08"},{"v":0.1318481,"d":"0.13"}]
["45009","Bamberg","SC",{"v":1.015595510663769,"d":"1.02"},{"v":1.015595510663769,"d":"1.02"},{"v":0.138474468,"d":"0.14"}]
["45011","Barnwell","SC",{"v":1.1084526186818344,"d":"1.11"},{"v":1.1084526186818342,"d":"1.11"},{"v":0.145965934,"d":"0.15"}]
["45013","Beaufort","SC",{"v":0.9778511093711445,"d":"0.98"},{"v":0.9778511093711445,"d":"0.98"},{"v":0.074011692,"d":"0.07"}]
["45015","Berkeley","SC",{"v":1.0217188658103364,"d":"1.02"},{"v":1.0217188658103364,"d":"1.02"},{"v":0.130449902,"d":"0.13"}]
["45017","Calhoun","SC",{"v":0.9863688745936473,"d":"0.99"},{"v":0.9863688745936473,"d":"0.99"},{"v":0.166030373,"d":"0.17"}]
["45019","Charleston","SC",{"v":0.9762655309601592,"d":"0.98"},{"v":0.9762655309601593,"d":"0.98"},{"v":0.079014158,"d":"0.08"}]
["45021","Cherokee","SC",{"v":1.1076311542803179,"d":"1.11"},{"v":1.1076311542803179,"d":"1.11"},{"v":0.183749221,"d":"0.18"}]
["45023","Chester","SC",{"v":0.9892418513340441,"d":"0.99"},{"v":0.9892418513340442,"d":"0.99"},{"v":0.167678746,"d":"0.17"}]
["45025","Chesterfield","SC",{"v":0.9762353035116007,"d":"0.98"},{"v":0.9762353035116008,"d":"0.98"},{"v":0.153900938,"d":"0.15"}]
["45027","Clarendon","SC",{"v":1.0508612684310892,"d":"1.05"},{"v":1.0508612684310892,"d":"1.05"},{"v":0.153677724,"d":"0.15"}]
["45029","Colleton","SC",{"v":1.0364076821492538,"d":"1.04"},{"v":1.0364076821492536,"d":"1.04"},{"v":0.14935269,"d":"0.15"}]
["45031","Darlington","SC",{"v":1.0720882236629763,"d":"1.07"},{"v":1.0720882236629763,"d":"1.07"},{"v":0.133013883,"d":"0.13"}]
["45033","Dillon","SC",{"v":1.0636062958038563,"d":"1.06"},{"v":1.0636062958038561,"d":"1.06"},{"v":0.15187351,"d":"0.15"}]
["45035","Dorchester","SC",{"v":0.991880268787069,"d":"0.99"},{"v":0.9918802687870689,"d":"0.99"},{"v":0.130637353,"d":"0.13"}]
["45037","Edgefield","SC",{"v":1.047290719899311,"d":"1.05"},{"v":1.047290719899311,"d":"1.05"},{"v":0.182275947,"d":"0.18"}]
["45039","Fairfield","SC",{"v":0.9915805159692026,"d":"0.99"},{"v":0.9915805159692027,"d":"0.99"},{"v":0.203685057,"d":"0.20"}]
["45041","Florence","SC",{"v":1.0239358791173911,"d":"1.02"},{"v":1.0239358791173911,"d":"1.02"},{"v":0.141181282,"d":"0.14"}]
["45043","Georgetown","SC",{"v":1.085948389972358,"d":"1.09"},{"v":1.085948389972358,"d":"1.09"},{"v":0.12095853500000002,"d":"0.12"}]
["45045","Greenville","SC",{"v":0.9903922854636756,"d":"0.99"},{"v":0.9903922854636755,"d":"0.99"},{"v":0.150854555,"d":"0.15"}]
["45047","Greenwood","SC",{"v":0.9755054613154037,"d":"0.98"},{"v":0.9755054613154036,"d":"0.98"},{"v":0.136571868,"d":"0.14"}]
["45049","Hampton","SC",{"v":1.0453913341353516,"d":"1.05"},{"v":1.0453913341353518,"d":"1.05"},{"v":0.160073151,"d":"0.16"}]
["45051","Horry","SC",{"v":0.9964918813049454,"d":"1.00"},{"v":0.9964918813049453,"d":"1.00"},{"v":0.128631223,"d":"0.13"}]
["45053","Jasper","SC",{"v":1.0407174320887376,"d":"1.04"},{"v":1.0407174320887373,"d":"1.04"},{"v":0.14453627,"d":"0.14"}]
["45055","Kershaw","SC",{"v":1.0466692219025204,"d":"1.05"},{"v":1.0466692219025202,"d":"1.05"},{"v":0.16516081,"d":"0.17"}]
["45057","Lancaster","SC",{"v":0.9246125050859693,"d":"0.92"},{"v":0.9246125050859693,"d":"0.92"},{"v":0.138033862,"d":"0.14"}]
["45059","Laurens","SC",{"v":1.0548441939957585,"d":"1.05"},{"v":1.0548441939957585,"d":"1.05"},{"v":0.169073568,"d":"0.17"}]
["45061","Lee","SC",{"v":1.1069378963788454,"d":"1.11"},{"v":1.1069378963788457,"d":"1.11"},{"v":0.140056168,"d":"0.14"}]
["45063","Lexington","SC",{"v":0.9748618998434205,"d":"0.97"},{"v":0.9748618998434204,"d":"0.97"},{"v":0.11797614299999999,"d":"0.12"}]
["45065","McCormick","SC",{"v":1.1061815992357715,"d":"1.11"},{"v":1.1061815992357715,"d":"1.11"},{"v":0.207066436,"d":"0.21"}]
["45067","Marion","SC",{"v":1.0076595080977067,"d":"1.01"},{"v":1.0076595080977067,"d":"1.01"},{"v":0.165488691,"d":"0.17"}]
["45069","Marlboro","SC",{"v":1.005019948284966,"d":"1.01"},{"v":1.0050199482849662,"d":"1.01"},{"v":0.140273966,"d":"0.14"}]
["45071","Newberry","SC",{"v":1.002268018937105,"d":"1.00"},{"v":1.002268018937105,"d":"1.00"},{"v":0.158600338,"d":"0.16"}]
["45073","Oconee","SC",{"v":1.1209469072521971,"d":"1.12"},{"v":1.120946907252197,"d":"1.12"},{"v":0.190363031,"d":"0.19"}]
["45075","Orangeburg","SC",{"v":0.9987653755023307,"d":"1.00"},{"v":0.9987653755023307,"d":"1.00"},{"v":0.144272553,"d":"0.14"}]
["45077","Pickens","SC",{"v":0.9520325213683195,"d":"0.95"},{"v":0.9520325213683195,"d":"0.95"},{"v":0.162005779,"d":"0.16"}]
["45079","Richland","SC",{"v":0.9229156060511303,"d":"0.92"},{"v":0.9229156060511302,"d":"0.92"},{"v":0.126601124,"d":"0.13"}]
["45081","Saluda","SC",{"v":1.0360423530152545,"d":"1.04"},{"v":1.0360423530152545,"d":"1.04"},{"v":0.170891248,"d":"0.17"}]
["45083","Spartanburg","SC",{"v":1.0208483396146901,"d":"1.02"},{"v":1.0208483396146903,"d":"1.02"},{"v":0.15170836,"d":"0.15"}]
["45085","Sumter","SC",{"v":0.9420905548469717,"d":"0.94"},{"v":0.9420905548469717,"d":"0.94"},{"v":0.13153902,"d":"0.13"}]
["45087","Union","SC",{"v":1.0506363357506188,"d":"1.05"},{"v":1.0506363357506188,"d":"1.05"},{"v":0.188130779,"d":"0.19"}]
["45089","Williamsburg","SC",{"v":1.0604349893931626,"d":"1.06"},{"v":1.0604349893931626,"d":"1.06"},{"v":0.180469295,"d":"0.18"}]
["45091","York","SC",{"v":0.9351809247307793,"d":"0.94"},{"v":0.9351809247307793,"d":"0.94"},{"v":0.133773758,"d":"0.13"}]
["46003","Aurora","SD",{"v":2.0653538761893753,"d":"2.07"},{"v":2.065353876189375,"d":"2.07"},{"v":0.597605599,"d":"0.60"}]
["46005","Beadle","SD",{"v":1.532206422716687,"d":"1.53"},{"v":1.532206422716687,"d":"1.53"},{"v":0.399927853,"d":"0.40"}]
["46007","Bennett","SD",{"v":2.122341258717096,"d":"2.12"},{"v":2.122341258717096,"d":"2.12"},{"v":0.533116019,"d":"0.53"}]
["46009","Bon Homme","SD",{"v":1.9764113645452241,"d":"1.98"},{"v":1.9764113645452241,"d":"1.98"},{"v":0.577471569,"d":"0.58"}]
["46011","Brookings","SD",{"v":1.9731307863024177,"d":"1.97"},{"v":1.973130786302418,"d":"1.97"},{"v":0.443642176,"d":"0.44"}]
["46013","Brown","SD",{"v":1.932168778819014,"d":"1.93"},{"v":1.9321687788190143,"d":"1.93"},{"v":0.440180843,"d":"0.44"}]
["46015","Brule","SD",{"v":1.7815330147688027,"d":"1.78"},{"v":1.7815330147688022,"d":"1.78"},{"v":0.620878363,"d":"0.62"}]
["46017","Buffalo","SD",{"v":1.4801943664381534,"d":"1.48"},{"v":1.4801943664381536,"d":"1.48"},{"v":0.624434007,"d":"0.62"}]
["46019","Butte","SD",{"v":1.8238464114423643,"d":"1.82"},{"v":1.8238464114423645,"d":"1.82"},{"v":0.443167184,"d":"0.44"}]
["46021","Campbell","SD",{"v":1.714831107658661,"d":"1.71"},{"v":1.7148311076586613,"d":"1.71"},{"v":0.764183562,"d":"0.76"}]
["46023","Charles Mix","SD",{"v":1.9713851803375122,"d":"1.97"},{"v":1.971385180337512,"d":"1.97"},{"v":0.603517868,"d":"0.60"}]
["46025","Clark","SD",{"v":2.0474760859652865,"d":"2.05"},{"v":2.0474760859652865,"d":"2.05"},{"v":0.55852653,"d":"0.56"}]
["46027","Clay","SD",{"v":1.8873197267650486,"d":"1.89"},{"v":1.8873197267650488,"d":"1.89"},{"v":0.334610163,"d":"0.33"}]
["46029","Codington","SD",{"v":1.751110198588725,"d":"1.75"},{"v":1.751110198588725,"d":"1.75"},{"v":0.374876679,"d":"0.37"}]
["46031","Corson","SD",{"v":2.146415053546296,"d":"2.15"},{"v":2.146415053546296,"d":"2.15"},{"v":0.77346772,"d":"0.77"}]
["46033","Custer","SD",{"v":2.129484467577098,"d":"2.13"},{"v":2.1294844675770976,"d":"2.13"},{"v":0.7401448700000001,"d":"0.74"}]
["46035","Davison","SD",{"v":1.8037772621774002,"d":"1.80"},{"v":1.8037772621774004,"d":"1.80"},{"v":0.30036167,"d":"0.30"}]
["46037","Day","SD",{"v":2.083324155601496,"d":"2.08"},{"v":2.083324155601496,"d":"2.08"},{"v":0.693414737,"d":"0.69"}]
["46039","Deuel","SD",{"v":1.83631329827278,"d":"1.84"},{"v":1.8363132982727797,"d":"1.84"},{"v":0.614840421,"d":"0.61"}]
["46041","Dewey","SD",{"v":2.043496630478864,"d":"2.04"},{"v":2.043496630478864,"d":"2.04"},{"v":0.697016828,"d":"0.70"}]
["46043","Douglas","SD",{"v":1.8484714334782548,"d":"1.85"},{"v":1.848471433478255,"d":"1.85"},{"v":0.589656724,"d":"0.59"}]
["46045","Edmunds","SD",{"v":1.8467799605978485,"d":"1.85"},{"v":1.8467799605978488,"d":"1.85"},{"v":0.633307202,"d":"0.63"}]
["46047","Fall River","SD",{"v":1.7547544572868605,"d":"1.75"},{"v":1.7547544572868605,"d":"1.75"},{"v":0.545579071,"d":"0.55"}]
["46049","Faulk","SD",{"v":2.133897136819067,"d":"2.13"},{"v":2.1338971368190665,"d":"2.13"},{"v":0.7533101859999999,"d":"0.75"}]
["46051","Grant","SD",{"v":2.0883672345676634,"d":"2.09"},{"v":2.088367234567664,"d":"2.09"},{"v":0.509130073,"d":"0.51"}]
["46053","Gregory","SD",{"v":2.0602325598454754,"d":"2.06"},{"v":2.060232559845476,"d":"2.06"},{"v":0.570409421,"d":"0.57"}]
["46055","Haakon","SD",{"v":2.0518820290543114,"d":"2.05"},{"v":2.0518820290543114,"d":"2.05"},{"v":0.539811106,"d":"0.54"}]
["46057","Hamlin","SD",{"v":1.6117932394961,"d":"1.61"},{"v":1.6117932394961003,"d":"1.61"},{"v":0.570458628,"d":"0.57"}]
["46059","Hand","SD",{"v":1.8482577755948466,"d":"1.85"},{"v":1.8482577755948468,"d":"1.85"},{"v":0.720578499,"d":"0.72"}]
["46061","Hanson","SD",{"v":1.8935958085981224,"d":"1.89"},{"v":1.8935958085981222,"d":"1.89"},{"v":0.531190527,"d":"0.53"}]
["46063","Harding","SD",{"v":2.145485312133064,"d":"2.15"},{"v":2.145485312133064,"d":"2.15"},{"v":0.678135547,"d":"0.68"}]
["46065","Hughes","SD",{"v":1.7850308944645832,"d":"1.79"},{"v":1.785030894464583,"d":"1.79"},{"v":0.353929515,"d":"0.35"}]
["46067","Hutchinson","SD",{"v":1.8747588819860033,"d":"1.87"},{"v":1.8747588819860035,"d":"1.87"},{"v":0.491844754,"d":"0.49"}]
["46069","Hyde","SD",{"v":1.988034107163955,"d":"1.99"},{"v":1.9880341071639551,"d":"1.99"},{"v":0.59588474,"d":"0.60"}]
["46071","Jackson","SD",{"v":1.5544538801954764,"d":"1.55"},{"v":1.5544538801954764,"d":"1.55"},{"v":0.537182875,"d":"0.54"}]
["46073","Jerauld","SD",{"v":1.8539668770160367,"d":"1.85"},{"v":1.8539668770160365,"d":"1.85"},{"v":0.711586719,"d":"0.71"}]
["46075","Jones","SD",{"v":2.081778476683138,"d":"2.08"},{"v":2.081778476683138,"d":"2.08"},{"v":0.62981331,"d":"0.63"}]
["46077","Kingsbury","SD",{"v":2.0319024103727066,"d":"2.03"},{"v":2.0319024103727066,"d":"2.03"},{"v":0.56377024,"d":"0.56"}]
["46079","Lake","SD",{"v":1.8043048722691577,"d":"1.80"},{"v":1.8043048722691575,"d":"1.80"},{"v":0.449179992,"d":"0.45"}]
["46081","Lawrence","SD",{"v":1.6457684000922945,"d":"1.65"},{"v":1.6457684000922943,"d":"1.65"},{"v":0.555710425,"d":"0.56"}]
["46083","Lincoln","SD",{"v":1.852235664428551,"d":"1.85"},{"v":1.852235664428551,"d":"1.85"},{"v":0.320705266,"d":"0.32"}]
["46085","Lyman","SD",{"v":1.9754406074647872,"d":"1.98"},{"v":1.9754406074647872,"d":"1.98"},{"v":0.626626568,"d":"0.63"}]
["46087","McCook","SD",{"v":1.6066248558131706,"d":"1.61"},{"v":1.6066248558131706,"d":"1.61"},{"v":0.47564252399999996,"d":"0.48"}]
["46089","McPherson","SD",{"v":1.8572751333023256,"d":"1.86"},{"v":1.8572751333023259,"d":"1.86"},{"v":0.748621188,"d":"0.75"}]
["46091","Marshall","SD",{"v":2.154670589930658,"d":"2.15"},{"v":2.154670589930658,"d":"2.15"},{"v":0.799193653,"d":"0.80"}]
["46093","Meade","SD",{"v":1.8889807162041417,"d":"1.89"},{"v":1.8889807162041414,"d":"1.89"},{"v":0.42351546400000006,"d":"0.42"}]
["46095","Mellette","SD",{"v":2.0503972404418893,"d":"2.05"},{"v":2.0503972404418893,"d":"2.05"},{"v":0.540179582,"d":"0.54"}]
["46097","Miner","SD",{"v":2.081906841474979,"d":"2.08"},{"v":2.081906841474979,"d":"2.08"},{"v":0.590013445,"d":"0.59"}]
["46099","Minnehaha","SD",{"v":1.744196529366098,"d":"1.74"},{"v":1.744196529366098,"d":"1.74"},{"v":0.29909688200000006,"d":"0.30"}]
["46101","Moody","SD",{"v":1.9767759328386199,"d":"1.98"},{"v":1.9767759328386199,"d":"1.98"},{"v":0.603645981,"d":"0.60"}]
["46102","Oglala Lakota","SD",{"v":1.9040000000000001,"d":"1.90"},{"v":1.9040000000000001,"d":"1.90"},{"v":0.5555715469076924,"d":"0.56"}]
["46103","Pennington","SD",{"v":1.5900938651228307,"d":"1.59"},{"v":1.590093865122831,"d":"1.59"},{"v":0.310127776,"d":"0.31"}]
["46105","Perkins","SD",{"v":1.6865428973145005,"d":"1.69"},{"v":1.6865428973145005,"d":"1.69"},{"v":0.692222732,"d":"0.69"}]
["46107","Potter","SD",{"v":2.1575324496626123,"d":"2.16"},{"v":2.1575324496626123,"d":"2.16"},{"v":0.629750649,"d":"0.63"}]
["46109","Roberts","SD",{"v":1.9512747869604505,"d":"1.95"},{"v":1.9512747869604505,"d":"1.95"},{"v":0.803306717,"d":"0.80"}]
["46111","Sanborn","SD",{"v":2.058561454309024,"d":"2.06"},{"v":2.058561454309024,"d":"2.06"},{"v":0.724582781,"d":"0.72"}]
["46115","Spink","SD",{"v":1.9923649053711643,"d":"1.99"},{"v":1.9923649053711643,"d":"1.99"},{"v":0.572226356,"d":"0.57"}]
["46117","Stanley","SD",{"v":1.8688282541297263,"d":"1.87"},{"v":1.868828254129726,"d":"1.87"},{"v":0.367335143,"d":"0.37"}]
["46119","Sully","SD",{"v":1.6478633938161105,"d":"1.65"},{"v":1.6478633938161107,"d":"1.65"},{"v":0.523690754,"d":"0.52"}]
["46121","Todd","SD",{"v":2.036174536820248,"d":"2.04"},{"v":2.036174536820248,"d":"2.04"},{"v":0.540979143,"d":"0.54"}]
["46123","Tripp","SD",{"v":2.03423208619171,"d":"2.03"},{"v":2.03423208619171,"d":"2.03"},{"v":0.450493654,"d":"0.45"}]
["46125","Turner","SD",{"v":1.9370023381255406,"d":"1.94"},{"v":1.9370023381255406,"d":"1.94"},{"v":0.497574773,"d":"0.50"}]
["46127","Union","SD",{"v":2.0105923700977177,"d":"2.01"},{"v":2.0105923700977177,"d":"2.01"},{"v":0.405336956,"d":"0.41"}]
["46129","Walworth","SD",{"v":2.102104243317112,"d":"2.10"},{"v":2.102104243317112,"d":"2.10"},{"v":0.46706362500000004,"d":"0.47"}]
["46135","Yankton","SD",{"v":1.8975803831018798,"d":"1.90"},{"v":1.8975803831018796,"d":"1.90"},{"v":0.35422413,"d":"0.35"}]
["46137","Ziebach","SD",{"v":1.84351067875869,"d":"1.84"},{"v":1.84351067875869,"d":"1.84"},{"v":0.680140592,"d":"0.68"}]
["47001","Anderson","TN",{"v":1.33721201177474,"d":"1.34"},{"v":1.3372120117747397,"d":"1.34"},{"v":0.271370194,"d":"0.27"}]
["47003","Bedford","TN",{"v":1.3800004125725998,"d":"1.38"},{"v":1.3800004125725995,"d":"1.38"},{"v":0.19498719,"d":"0.19"}]
["47005","Benton","TN",{"v":1.540793783666407,"d":"1.54"},{"v":1.5407937836664072,"d":"1.54"},{"v":0.250051567,"d":"0.25"}]
["47007","Bledsoe","TN",{"v":1.4842335645388915,"d":"1.48"},{"v":1.4842335645388913,"d":"1.48"},{"v":0.346115955,"d":"0.35"}]
["47009","Blount","TN",{"v":1.437801510524501,"d":"1.44"},{"v":1.4378015105245008,"d":"1.44"},{"v":0.279510512,"d":"0.28"}]
["47011","Bradley","TN",{"v":1.3171127940952374,"d":"1.32"},{"v":1.3171127940952374,"d":"1.32"},{"v":0.265783692,"d":"0.27"}]
["47013","Campbell","TN",{"v":1.4751260285765486,"d":"1.48"},{"v":1.4751260285765484,"d":"1.48"},{"v":0.341791662,"d":"0.34"}]
["47015","Cannon","TN",{"v":1.406797002169713,"d":"1.41"},{"v":1.406797002169713,"d":"1.41"},{"v":0.250492619,"d":"0.25"}]
["47017","Carroll","TN",{"v":1.5159257035118174,"d":"1.52"},{"v":1.5159257035118177,"d":"1.52"},{"v":0.217029035,"d":"0.22"}]
["47019","Carter","TN",{"v":1.3938524281857436,"d":"1.39"},{"v":1.3938524281857434,"d":"1.39"},{"v":0.364734321,"d":"0.36"}]
["47021","Cheatham","TN",{"v":1.6789950163565712,"d":"1.68"},{"v":1.6789950163565712,"d":"1.68"},{"v":0.309716789,"d":"0.31"}]
["47023","Chester","TN",{"v":1.515670560713988,"d":"1.52"},{"v":1.515670560713988,"d":"1.52"},{"v":0.226189595,"d":"0.23"}]
["47025","Claiborne","TN",{"v":1.7250470688282784,"d":"1.73"},{"v":1.7250470688282784,"d":"1.73"},{"v":0.350862342,"d":"0.35"}]
["47027","Clay","TN",{"v":1.4727743748339768,"d":"1.47"},{"v":1.4727743748339768,"d":"1.47"},{"v":0.357088449,"d":"0.36"}]
["47029","Cocke","TN",{"v":1.5227861767419093,"d":"1.52"},{"v":1.5227861767419093,"d":"1.52"},{"v":0.364449948,"d":"0.36"}]
["47031","Coffee","TN",{"v":1.4584916760965205,"d":"1.46"},{"v":1.4584916760965205,"d":"1.46"},{"v":0.218703469,"d":"0.22"}]
["47033","Crockett","TN",{"v":1.316486592819395,"d":"1.32"},{"v":1.316486592819395,"d":"1.32"},{"v":0.149788517,"d":"0.15"}]
["47035","Cumberland","TN",{"v":1.3891168507821594,"d":"1.39"},{"v":1.3891168507821594,"d":"1.39"},{"v":0.28953302799999997,"d":"0.29"}]
["47037","Davidson","TN",{"v":0.5666630901250872,"d":"0.57"},{"v":0.5666630901250873,"d":"0.57"},{"v":0.292337312,"d":"0.29"}]
["47039","Decatur","TN",{"v":1.4778403042874502,"d":"1.48"},{"v":1.47784030428745,"d":"1.48"},{"v":0.245799569,"d":"0.25"}]
["47041","Dekalb","TN",{"v":1.078476426903936,"d":"1.08"},{"v":1.0784764269039357,"d":"1.08"},{"v":0.222953326,"d":"0.22"}]
["47043","Dickson","TN",{"v":1.456972722741105,"d":"1.46"},{"v":1.4569727227411047,"d":"1.46"},{"v":0.227547082,"d":"0.23"}]
["47045","Dyer","TN",{"v":1.0771165221236474,"d":"1.08"},{"v":1.0771165221236474,"d":"1.08"},{"v":0.127998997,"d":"0.13"}]
["47047","Fayette","TN",{"v":1.513769463871124,"d":"1.51"},{"v":1.513769463871124,"d":"1.51"},{"v":0.188643331,"d":"0.19"}]
["47049","Fentress","TN",{"v":1.5726595948956406,"d":"1.57"},{"v":1.5726595948956408,"d":"1.57"},{"v":0.38976743599999997,"d":"0.39"}]
["47051","Franklin","TN",{"v":1.500337525991214,"d":"1.50"},{"v":1.5003375259912142,"d":"1.50"},{"v":0.280651909,"d":"0.28"}]
["47053","Gibson","TN",{"v":1.5221222794670028,"d":"1.52"},{"v":1.5221222794670028,"d":"1.52"},{"v":0.138001157,"d":"0.14"}]
["47055","Giles","TN",{"v":1.4981969297215139,"d":"1.50"},{"v":1.4981969297215139,"d":"1.50"},{"v":0.24011416,"d":"0.24"}]
["47057","Grainger","TN",{"v":1.3900319607939264,"d":"1.39"},{"v":1.3900319607939267,"d":"1.39"},{"v":0.340265038,"d":"0.34"}]
["47059","Greene","TN",{"v":1.4545062727319016,"d":"1.45"},{"v":1.4545062727319016,"d":"1.45"},{"v":0.26356133,"d":"0.26"}]
["47061","Grundy","TN",{"v":1.6547043042217235,"d":"1.65"},{"v":1.6547043042217238,"d":"1.65"},{"v":0.416878887,"d":"0.42"}]
["47063","Hamblen","TN",{"v":1.317328778201295,"d":"1.32"},{"v":1.3173287782012952,"d":"1.32"},{"v":0.20202746,"d":"0.20"}]
["47065","Hamilton","TN",{"v":1.2920543667832365,"d":"1.29"},{"v":1.2920543667832365,"d":"1.29"},{"v":0.266951912,"d":"0.27"}]
["47067","Hancock","TN",{"v":1.6751832583491966,"d":"1.68"},{"v":1.6751832583491968,"d":"1.68"},{"v":0.390903196,"d":"0.39"}]
["47069","Hardeman","TN",{"v":1.485575805320222,"d":"1.49"},{"v":1.4855758053202222,"d":"1.49"},{"v":0.253951075,"d":"0.25"}]
["47071","Hardin","TN",{"v":1.428854260744431,"d":"1.43"},{"v":1.4288542607444308,"d":"1.43"},{"v":0.241878476,"d":"0.24"}]
["47073","Hawkins","TN",{"v":1.652011499431141,"d":"1.65"},{"v":1.6520114994311412,"d":"1.65"},{"v":0.280254954,"d":"0.28"}]
["47075","Haywood","TN",{"v":1.5267701045658018,"d":"1.53"},{"v":1.5267701045658018,"d":"1.53"},{"v":0.142314277,"d":"0.14"}]
["47077","Henderson","TN",{"v":1.4750485226724674,"d":"1.48"},{"v":1.4750485226724677,"d":"1.48"},{"v":0.19554235499999997,"d":"0.20"}]
["47079","Henry","TN",{"v":1.4755908534132647,"d":"1.48"},{"v":1.475590853413265,"d":"1.48"},{"v":0.207973765,"d":"0.21"}]
["47081","Hickman","TN",{"v":1.5717039669650386,"d":"1.57"},{"v":1.5717039669650386,"d":"1.57"},{"v":0.327587653,"d":"0.33"}]
["47083","Houston","TN",{"v":1.6083998667485733,"d":"1.61"},{"v":1.608399866748573,"d":"1.61"},{"v":0.343097147,"d":"0.34"}]
["47085","Humphreys","TN",{"v":1.5274671221474025,"d":"1.53"},{"v":1.5274671221474025,"d":"1.53"},{"v":0.247831297,"d":"0.25"}]
["47087","Jackson","TN",{"v":1.57274091516158,"d":"1.57"},{"v":1.5727409151615799,"d":"1.57"},{"v":0.37469063,"d":"0.37"}]
["47089","Jefferson","TN",{"v":1.5245132394887655,"d":"1.52"},{"v":1.5245132394887655,"d":"1.52"},{"v":0.237213289,"d":"0.24"}]
["47091","Johnson","TN",{"v":1.481446914749249,"d":"1.48"},{"v":1.481446914749249,"d":"1.48"},{"v":0.435475172,"d":"0.44"}]
["47093","Knox","TN",{"v":1.2140001532658096,"d":"1.21"},{"v":1.2140001532658096,"d":"1.21"},{"v":0.25861452,"d":"0.26"}]
["47095","Lake","TN",{"v":1.2662928039501637,"d":"1.27"},{"v":1.2662928039501637,"d":"1.27"},{"v":0.156587141,"d":"0.16"}]
["47097","Lauderdale","TN",{"v":1.350070466115271,"d":"1.35"},{"v":1.350070466115271,"d":"1.35"},{"v":0.145475124,"d":"0.15"}]
["47099","Lawrence","TN",{"v":1.4359617773182838,"d":"1.44"},{"v":1.435961777318284,"d":"1.44"},{"v":0.22547651399999996,"d":"0.23"}]
["47101","Lewis","TN",{"v":1.6117208505368736,"d":"1.61"},{"v":1.6117208505368734,"d":"1.61"},{"v":0.271683602,"d":"0.27"}]
["47103","Lincoln","TN",{"v":1.3763844794320916,"d":"1.38"},{"v":1.3763844794320916,"d":"1.38"},{"v":0.205497028,"d":"0.21"}]
["47105","Loudon","TN",{"v":1.3683332242007942,"d":"1.37"},{"v":1.3683332242007944,"d":"1.37"},{"v":0.20617295499999996,"d":"0.21"}]
["47107","McMinn","TN",{"v":1.3833972266804537,"d":"1.38"},{"v":1.3833972266804537,"d":"1.38"},{"v":0.24880305900000002,"d":"0.25"}]
["47109","McNairy","TN",{"v":1.5365639224832324,"d":"1.54"},{"v":1.5365639224832324,"d":"1.54"},{"v":0.304797039,"d":"0.30"}]
["47111","Macon","TN",{"v":1.369088661719402,"d":"1.37"},{"v":1.369088661719402,"d":"1.37"},{"v":0.277552029,"d":"0.28"}]
["47113","Madison","TN",{"v":1.3796855433528408,"d":"1.38"},{"v":1.3796855433528405,"d":"1.38"},{"v":0.162629056,"d":"0.16"}]
["47115","Marion","TN",{"v":1.6101992542984582,"d":"1.61"},{"v":1.6101992542984582,"d":"1.61"},{"v":0.378117274,"d":"0.38"}]
["47117","Marshall","TN",{"v":1.6200833822633727,"d":"1.62"},{"v":1.6200833822633727,"d":"1.62"},{"v":0.215987139,"d":"0.22"}]
["47119","Maury","TN",{"v":1.4263662112557098,"d":"1.43"},{"v":1.42636621125571,"d":"1.43"},{"v":0.192704789,"d":"0.19"}]
["47121","Meigs","TN",{"v":1.378931509988729,"d":"1.38"},{"v":1.378931509988729,"d":"1.38"},{"v":0.321781206,"d":"0.32"}]
["47123","Monroe","TN",{"v":1.4146626735210686,"d":"1.41"},{"v":1.4146626735210686,"d":"1.41"},{"v":0.369342012,"d":"0.37"}]
["47125","Montgomery","TN",{"v":1.5293663216743183,"d":"1.53"},{"v":1.529366321674318,"d":"1.53"},{"v":0.207634712,"d":"0.21"}]
["47127","Moore","TN",{"v":1.65699723841521,"d":"1.66"},{"v":1.6569972384152098,"d":"1.66"},{"v":0.273668281,"d":"0.27"}]
["47129","Morgan","TN",{"v":1.529408642256583,"d":"1.53"},{"v":1.529408642256583,"d":"1.53"},{"v":0.376113547,"d":"0.38"}]
["47131","Obion","TN",{"v":1.376568069096718,"d":"1.38"},{"v":1.3765680690967177,"d":"1.38"},{"v":0.146096203,"d":"0.15"}]
["47133","Overton","TN",{"v":1.306668434778279,"d":"1.31"},{"v":1.3066684347782787,"d":"1.31"},{"v":0.358351937,"d":"0.36"}]
["47135","Perry","TN",{"v":1.6271747395744693,"d":"1.63"},{"v":1.6271747395744693,"d":"1.63"},{"v":0.336653763,"d":"0.34"}]
["47137","Pickett","TN",{"v":1.607665441100358,"d":"1.61"},{"v":1.607665441100358,"d":"1.61"},{"v":0.40811401199999997,"d":"0.41"}]
["47139","Polk","TN",{"v":1.408820131719186,"d":"1.41"},{"v":1.4088201317191857,"d":"1.41"},{"v":0.460690404,"d":"0.46"}]
["47141","Putnam","TN",{"v":1.4541583553328146,"d":"1.45"},{"v":1.4541583553328146,"d":"1.45"},{"v":0.27859859,"d":"0.28"}]
["47143","Rhea","TN",{"v":1.4489768847417235,"d":"1.45"},{"v":1.4489768847417235,"d":"1.45"},{"v":0.267073564,"d":"0.27"}]
["47145","Roane","TN",{"v":1.3703654294814538,"d":"1.37"},{"v":1.3703654294814536,"d":"1.37"},{"v":0.25525699,"d":"0.26"}]
["47147","Robertson","TN",{"v":1.3533071385341537,"d":"1.35"},{"v":1.3533071385341537,"d":"1.35"},{"v":0.170992281,"d":"0.17"}]
["47149","Rutherford","TN",{"v":1.4372403028621425,"d":"1.44"},{"v":1.4372403028621423,"d":"1.44"},{"v":0.184966007,"d":"0.18"}]
["47151","Scott","TN",{"v":1.4474687710222762,"d":"1.45"},{"v":1.4474687710222762,"d":"1.45"},{"v":0.333484883,"d":"0.33"}]
["47153","Sequatchie","TN",{"v":1.5233365374358225,"d":"1.52"},{"v":1.523336537435823,"d":"1.52"},{"v":0.390151555,"d":"0.39"}]
["47155","Sevier","TN",{"v":1.4061653985653382,"d":"1.41"},{"v":1.4061653985653382,"d":"1.41"},{"v":0.383767632,"d":"0.38"}]
["47157","Shelby","TN",{"v":0.746017664216711,"d":"0.75"},{"v":0.7460176642167109,"d":"0.75"},{"v":0.21702354,"d":"0.22"}]
["47159","Smith","TN",{"v":1.2869109844932993,"d":"1.29"},{"v":1.2869109844932995,"d":"1.29"},{"v":0.246524568,"d":"0.25"}]
["47161","Stewart","TN",{"v":1.6179795560435006,"d":"1.62"},{"v":1.6179795560435009,"d":"1.62"},{"v":0.35446266,"d":"0.35"}]
["47163","Sullivan","TN",{"v":1.3756938830699275,"d":"1.38"},{"v":1.3756938830699275,"d":"1.38"},{"v":0.273555016,"d":"0.27"}]
["47165","Sumner","TN",{"v":1.4184397263486805,"d":"1.42"},{"v":1.4184397263486805,"d":"1.42"},{"v":0.174882454,"d":"0.17"}]
["47167","Tipton","TN",{"v":1.1907176237340231,"d":"1.19"},{"v":1.1907176237340233,"d":"1.19"},{"v":0.142551695,"d":"0.14"}]
["47169","Trousdale","TN",{"v":1.549478494119015,"d":"1.55"},{"v":1.549478494119015,"d":"1.55"},{"v":0.245905161,"d":"0.25"}]
["47171","Unicoi","TN",{"v":1.3620747464757825,"d":"1.36"},{"v":1.3620747464757825,"d":"1.36"},{"v":0.341562777,"d":"0.34"}]
["47173","Union","TN",{"v":1.3490139736992304,"d":"1.35"},{"v":1.3490139736992302,"d":"1.35"},{"v":0.362749282,"d":"0.36"}]
["47175","Van Buren","TN",{"v":1.5256303293575482,"d":"1.53"},{"v":1.5256303293575484,"d":"1.53"},{"v":0.37341151300000003,"d":"0.37"}]
["47177","Warren","TN",{"v":1.5330406835941734,"d":"1.53"},{"v":1.5330406835941734,"d":"1.53"},{"v":0.22585985,"d":"0.23"}]
["47179","Washington","TN",{"v":1.4093013897921671,"d":"1.41"},{"v":1.4093013897921671,"d":"1.41"},{"v":0.223288883,"d":"0.22"}]
["47181","Wayne","TN",{"v":1.5783102726642853,"d":"1.58"},{"v":1.578310272664285,"d":"1.58"},{"v":0.346506325,"d":"0.35"}]
["47183","Weakley","TN",{"v":1.5153382733279923,"d":"1.52"},{"v":1.5153382733279923,"d":"1.52"},{"v":0.187304906,"d":"0.19"}]
["47185","White","TN",{"v":1.4929543650034174,"d":"1.49"},{"v":1.4929543650034174,"d":"1.49"},{"v":0.254462278,"d":"0.25"}]
["47187","Williamson","TN",{"v":1.3962913536319288,"d":"1.40"},{"v":1.396291353631929,"d":"1.40"},{"v":0.165883764,"d":"0.17"}]
["47189","Wilson","TN",{"v":1.2888385221172964,"d":"1.29"},{"v":1.2888385221172967,"d":"1.29"},{"v":0.17966560800000003,"d":"0.18"}]
["48001","Anderson","TX",{"v":1.1781516003157946,"d":"1.18"},{"v":1.1781516003157946,"d":"1.18"},{"v":0.144692174,"d":"0.14"}]
["48003","Andrews","TX",{"v":1.2541167282991141,"d":"1.25"},{"v":1.2541167282991141,"d":"1.25"},{"v":0.080532277,"d":"0.08"}]
["48005","Angelina","TX",{"v":1.183048666099328,"d":"1.18"},{"v":1.1830486660993278,"d":"1.18"},{"v":0.149867026,"d":"0.15"}]
["48007","Aransas","TX",{"v":1.1280533893722324,"d":"1.13"},{"v":1.1280533893722327,"d":"1.13"},{"v":0.055327092999999994,"d":"0.06"}]
["48009","Archer","TX",{"v":1.1940560692049975,"d":"1.19"},{"v":1.1940560692049975,"d":"1.19"},{"v":0.093090992,"d":"0.09"}]
["48011","Armstrong","TX",{"v":1.1891950142079895,"d":"1.19"},{"v":1.1891950142079895,"d":"1.19"},{"v":0.0971055,"d":"0.10"}]
["48013","Atascosa","TX",{"v":1.1470726822143034,"d":"1.15"},{"v":1.1470726822143031,"d":"1.15"},{"v":0.074716654,"d":"0.07"}]
["48015","Austin","TX",{"v":1.1370948164580126,"d":"1.14"},{"v":1.1370948164580126,"d":"1.14"},{"v":0.082032725,"d":"0.08"}]
["48017","Bailey","TX",{"v":1.226843609604067,"d":"1.23"},{"v":1.226843609604067,"d":"1.23"},{"v":0.077338576,"d":"0.08"}]
["48019","Bandera","TX",{"v":1.2545759407296944,"d":"1.25"},{"v":1.2545759407296941,"d":"1.25"},{"v":0.166046462,"d":"0.17"}]
["48021","Bastrop","TX",{"v":1.1599925858514102,"d":"1.16"},{"v":1.1599925858514102,"d":"1.16"},{"v":0.1031734,"d":"0.10"}]
["48023","Baylor","TX",{"v":1.1443411681781752,"d":"1.14"},{"v":1.1443411681781752,"d":"1.14"},{"v":0.087122219,"d":"0.09"}]
["48025","Bee","TX",{"v":1.117809159917925,"d":"1.12"},{"v":1.117809159917925,"d":"1.12"},{"v":0.071402125,"d":"0.07"}]
["48027","Bell","TX",{"v":1.161303431297424,"d":"1.16"},{"v":1.1613034312974242,"d":"1.16"},{"v":0.100612108,"d":"0.10"}]
["48029","Bexar","TX",{"v":0.5288804746278346,"d":"0.53"},{"v":0.5288804746278345,"d":"0.53"},{"v":0.12491640100000001,"d":"0.12"}]
["48031","Blanco","TX",{"v":1.219812523343642,"d":"1.22"},{"v":1.219812523343642,"d":"1.22"},{"v":0.131403536,"d":"0.13"}]
["48033","Borden","TX",{"v":1.2612834845069718,"d":"1.26"},{"v":1.2612834845069718,"d":"1.26"},{"v":0.121332543,"d":"0.12"}]
["48035","Bosque","TX",{"v":1.203353763149956,"d":"1.20"},{"v":1.203353763149956,"d":"1.20"},{"v":0.12210820000000001,"d":"0.12"}]
["48037","Bowie","TX",{"v":1.2242006766092834,"d":"1.22"},{"v":1.2242006766092837,"d":"1.22"},{"v":0.106687303,"d":"0.11"}]
["48039","Brazoria","TX",{"v":1.070537326333775,"d":"1.07"},{"v":1.0705373263337752,"d":"1.07"},{"v":0.05594478,"d":"0.06"}]
["48041","Brazos","TX",{"v":1.0913494683849316,"d":"1.09"},{"v":1.0913494683849319,"d":"1.09"},{"v":0.087702536,"d":"0.09"}]
["48043","Brewster","TX",{"v":1.1462027592120372,"d":"1.15"},{"v":1.146202759212037,"d":"1.15"},{"v":0.070091452,"d":"0.07"}]
["48045","Briscoe","TX",{"v":1.181207273682589,"d":"1.18"},{"v":1.181207273682589,"d":"1.18"},{"v":0.104512534,"d":"0.10"}]
["48047","Brooks","TX",{"v":1.1042285880998521,"d":"1.10"},{"v":1.1042285880998524,"d":"1.10"},{"v":0.05870103,"d":"0.06"}]
["48049","Brown","TX",{"v":1.1814845135039904,"d":"1.18"},{"v":1.1814845135039906,"d":"1.18"},{"v":0.093468173,"d":"0.09"}]
["48051","Burleson","TX",{"v":1.1745122726320147,"d":"1.17"},{"v":1.1745122726320152,"d":"1.17"},{"v":0.094073942,"d":"0.09"}]
["48053","Burnet","TX",{"v":1.207984974084771,"d":"1.21"},{"v":1.207984974084771,"d":"1.21"},{"v":0.11278182599999999,"d":"0.11"}]
["48055","Caldwell","TX",{"v":1.131455649929615,"d":"1.13"},{"v":1.131455649929615,"d":"1.13"},{"v":0.081033305,"d":"0.08"}]
["48057","Calhoun","TX",{"v":1.1166423469912352,"d":"1.12"},{"v":1.1166423469912352,"d":"1.12"},{"v":0.05581269,"d":"0.06"}]
["48059","Callahan","TX",{"v":1.2211101271544078,"d":"1.22"},{"v":1.2211101271544078,"d":"1.22"},{"v":0.10871772599999999,"d":"0.11"}]
["48061","Cameron","TX",{"v":1.0695738893414117,"d":"1.07"},{"v":1.0695738893414117,"d":"1.07"},{"v":0.051853863,"d":"0.05"}]
["48063","Camp","TX",{"v":1.2633789281953915,"d":"1.26"},{"v":1.2633789281953913,"d":"1.26"},{"v":0.131680767,"d":"0.13"}]
["48065","Carson","TX",{"v":1.1950627556759081,"d":"1.20"},{"v":1.1950627556759084,"d":"1.20"},{"v":0.090671495,"d":"0.09"}]
["48067","Cass","TX",{"v":1.2111054206247922,"d":"1.21"},{"v":1.2111054206247922,"d":"1.21"},{"v":0.16853677099999997,"d":"0.17"}]
["48069","Castro","TX",{"v":1.1819836819453564,"d":"1.18"},{"v":1.1819836819453566,"d":"1.18"},{"v":0.076634944,"d":"0.08"}]
["48071","Chambers","TX",{"v":1.2166678313073487,"d":"1.22"},{"v":1.2166678313073487,"d":"1.22"},{"v":0.061004872,"d":"0.06"}]
["48073","Cherokee","TX",{"v":1.1977234924066797,"d":"1.20"},{"v":1.1977234924066797,"d":"1.20"},{"v":0.147660327,"d":"0.15"}]
["48075","Childress","TX",{"v":1.1629751189693374,"d":"1.16"},{"v":1.1629751189693374,"d":"1.16"},{"v":0.062193221,"d":"0.06"}]
["48077","Clay","TX",{"v":1.2015202866076036,"d":"1.20"},{"v":1.2015202866076036,"d":"1.20"},{"v":0.09151657,"d":"0.09"}]
["48079","Cochran","TX",{"v":1.1689405047582808,"d":"1.17"},{"v":1.1689405047582808,"d":"1.17"},{"v":0.086878229,"d":"0.09"}]
["48081","Coke","TX",{"v":1.185934834902335,"d":"1.19"},{"v":1.185934834902335,"d":"1.19"},{"v":0.106996654,"d":"0.11"}]
["48083","Coleman","TX",{"v":1.1753175549420851,"d":"1.18"},{"v":1.1753175549420851,"d":"1.18"},{"v":0.091310104,"d":"0.09"}]
["48085","Collin","TX",{"v":0.8679653859031502,"d":"0.87"},{"v":0.8679653859031502,"d":"0.87"},{"v":0.103941526,"d":"0.10"}]
["48087","Collingsworth","TX",{"v":1.1269421025945863,"d":"1.13"},{"v":1.126942102594586,"d":"1.13"},{"v":0.081833799,"d":"0.08"}]
["48089","Colorado","TX",{"v":1.1281229996407427,"d":"1.13"},{"v":1.1281229996407427,"d":"1.13"},{"v":0.081367666,"d":"0.08"}]
["48091","Comal","TX",{"v":1.1344551836126204,"d":"1.13"},{"v":1.1344551836126204,"d":"1.13"},{"v":0.105959699,"d":"0.11"}]
["48093","Comanche","TX",{"v":1.212036468549421,"d":"1.21"},{"v":1.212036468549421,"d":"1.21"},{"v":0.108992802,"d":"0.11"}]
["48095","Concho","TX",{"v":1.1668392305732238,"d":"1.17"},{"v":1.1668392305732238,"d":"1.17"},{"v":0.087303982,"d":"0.09"}]
["48097","Cooke","TX",{"v":1.1872617014369449,"d":"1.19"},{"v":1.187261701436945,"d":"1.19"},{"v":0.098810372,"d":"0.10"}]
["48099","Coryell","TX",{"v":1.1693106371838082,"d":"1.17"},{"v":1.1693106371838082,"d":"1.17"},{"v":0.092010149,"d":"0.09"}]
["48101","Cottle","TX",{"v":1.1000409206776625,"d":"1.10"},{"v":1.1000409206776625,"d":"1.10"},{"v":0.091280542,"d":"0.09"}]
["48103","Crane","TX",{"v":1.1459798467115743,"d":"1.15"},{"v":1.1459798467115743,"d":"1.15"},{"v":0.05128795500000001,"d":"0.05"}]
["48105","Crockett","TX",{"v":1.1520446544874101,"d":"1.15"},{"v":1.1520446544874101,"d":"1.15"},{"v":0.065814651,"d":"0.07"}]
["48107","Crosby","TX",{"v":1.175098080563602,"d":"1.18"},{"v":1.175098080563602,"d":"1.18"},{"v":0.098525172,"d":"0.10"}]
["48109","Culberson","TX",{"v":1.0882026200186885,"d":"1.09"},{"v":1.0882026200186887,"d":"1.09"},{"v":0.067854535,"d":"0.07"}]
["48111","Dallam","TX",{"v":1.195134605506214,"d":"1.20"},{"v":1.195134605506214,"d":"1.20"},{"v":0.069073133,"d":"0.07"}]
["48113","Dallas","TX",{"v":5.1136273583668795E-3,"d":"0.01"},{"v":0.00511362735836688,"d":"0.01"},{"v":0.323572049,"d":"0.32"}]
["48115","Dawson","TX",{"v":1.1810260871395692,"d":"1.18"},{"v":1.181026087139569,"d":"1.18"},{"v":0.066372218,"d":"0.07"}]
["48117","Deaf Smith","TX",{"v":1.1722516217040133,"d":"1.17"},{"v":1.1722516217040133,"d":"1.17"},{"v":0.063413027,"d":"0.06"}]
["48119","Delta","TX",{"v":1.1898485553296596,"d":"1.19"},{"v":1.1898485553296596,"d":"1.19"},{"v":0.111871024,"d":"0.11"}]
["48121","Denton","TX",{"v":1.0007538161544682,"d":"1.00"},{"v":1.0007538161544682,"d":"1.00"},{"v":0.094142084,"d":"0.09"}]
["48123","De Witt","TX",{"v":1.12045263250674,"d":"1.12"},{"v":1.1204526325067399,"d":"1.12"},{"v":0.079268374,"d":"0.08"}]
["48125","Dickens","TX",{"v":1.2285745266274404,"d":"1.23"},{"v":1.2285745266274404,"d":"1.23"},{"v":0.11692005400000001,"d":"0.12"}]
["48127","Dimmit","TX",{"v":1.1179508006103862,"d":"1.12"},{"v":1.117950800610386,"d":"1.12"},{"v":0.060165931,"d":"0.06"}]
["48129","Donley","TX",{"v":1.171284777773881,"d":"1.17"},{"v":1.171284777773881,"d":"1.17"},{"v":0.090328849,"d":"0.09"}]
["48131","Duval","TX",{"v":1.1111100230733764,"d":"1.11"},{"v":1.1111100230733761,"d":"1.11"},{"v":0.072865823,"d":"0.07"}]
["48133","Eastland","TX",{"v":1.1856096048919758,"d":"1.19"},{"v":1.1856096048919758,"d":"1.19"},{"v":0.104259315,"d":"0.10"}]
["48135","Ector","TX",{"v":1.147453002560781,"d":"1.15"},{"v":1.147453002560781,"d":"1.15"},{"v":0.054319871,"d":"0.05"}]
["48137","Edwards","TX",{"v":1.2292389369916024,"d":"1.23"},{"v":1.2292389369916024,"d":"1.23"},{"v":0.12681857,"d":"0.13"}]
["48139","Ellis","TX",{"v":1.1830124815212766,"d":"1.18"},{"v":1.1830124815212766,"d":"1.18"},{"v":0.089130167,"d":"0.09"}]
["48141","El Paso","TX",{"v":0.9665816252638157,"d":"0.97"},{"v":0.9665816252638156,"d":"0.97"},{"v":0.059713630000000004,"d":"0.06"}]
["48143","Erath","TX",{"v":1.211766565183445,"d":"1.21"},{"v":1.211766565183445,"d":"1.21"},{"v":0.10569363800000002,"d":"0.11"}]
["48145","Falls","TX",{"v":1.1777850242723926,"d":"1.18"},{"v":1.1777850242723926,"d":"1.18"},{"v":0.087053861,"d":"0.09"}]
["48147","Fannin","TX",{"v":1.1894265487063376,"d":"1.19"},{"v":1.1894265487063376,"d":"1.19"},{"v":0.11236294699999999,"d":"0.11"}]
["48149","Fayette","TX",{"v":1.1383258876530356,"d":"1.14"},{"v":1.1383258876530356,"d":"1.14"},{"v":0.08310399,"d":"0.08"}]
["48151","Fisher","TX",{"v":1.157253168103523,"d":"1.16"},{"v":1.157253168103523,"d":"1.16"},{"v":0.10600649599999999,"d":"0.11"}]
["48153","Floyd","TX",{"v":1.1748427385431564,"d":"1.17"},{"v":1.1748427385431566,"d":"1.17"},{"v":0.080456481,"d":"0.08"}]
["48155","Foard","TX",{"v":1.1464558774759022,"d":"1.15"},{"v":1.146455877475902,"d":"1.15"},{"v":0.097046928,"d":"0.10"}]
["48157","Fort Bend","TX",{"v":0.9550526657130257,"d":"0.96"},{"v":0.9550526657130258,"d":"0.96"},{"v":0.059151596,"d":"0.06"}]
["48159","Franklin","TX",{"v":1.219835671208657,"d":"1.22"},{"v":1.219835671208657,"d":"1.22"},{"v":0.118016871,"d":"0.12"}]
["48161","Freestone","TX",{"v":1.2103633938855898,"d":"1.21"},{"v":1.2103633938855898,"d":"1.21"},{"v":0.120048367,"d":"0.12"}]
["48163","Frio","TX",{"v":1.1272921065390402,"d":"1.13"},{"v":1.1272921065390402,"d":"1.13"},{"v":0.060887037,"d":"0.06"}]
["48165","Gaines","TX",{"v":1.252223867237354,"d":"1.25"},{"v":1.252223867237354,"d":"1.25"},{"v":0.10060917100000001,"d":"0.10"}]
["48167","Galveston","TX",{"v":0.9224030446273626,"d":"0.92"},{"v":0.9224030446273626,"d":"0.92"},{"v":0.056811359,"d":"0.06"}]
["48169","Garza","TX",{"v":1.1593559422381143,"d":"1.16"},{"v":1.1593559422381143,"d":"1.16"},{"v":0.070596647,"d":"0.07"}]
["48171","Gillespie","TX",{"v":1.1763794935683494,"d":"1.18"},{"v":1.1763794935683491,"d":"1.18"},{"v":0.104172432,"d":"0.10"}]
["48173","Glasscock","TX",{"v":1.2939356633053964,"d":"1.29"},{"v":1.2939356633053962,"d":"1.29"},{"v":0.139915415,"d":"0.14"}]
["48175","Goliad","TX",{"v":1.1550414772675834,"d":"1.16"},{"v":1.1550414772675832,"d":"1.16"},{"v":0.100580642,"d":"0.10"}]
["48177","Gonzales","TX",{"v":1.1452512482398538,"d":"1.15"},{"v":1.1452512482398538,"d":"1.15"},{"v":0.08669436,"d":"0.09"}]
["48179","Gray","TX",{"v":1.1621563266920387,"d":"1.16"},{"v":1.1621563266920387,"d":"1.16"},{"v":0.06257879,"d":"0.06"}]
["48181","Grayson","TX",{"v":1.1519278691059174,"d":"1.15"},{"v":1.1519278691059172,"d":"1.15"},{"v":0.094298049,"d":"0.09"}]
["48183","Gregg","TX",{"v":1.1883867258636964,"d":"1.19"},{"v":1.1883867258636962,"d":"1.19"},{"v":0.11902462100000001,"d":"0.12"}]
["48185","Grimes","TX",{"v":1.108710680630682,"d":"1.11"},{"v":1.1087106806306821,"d":"1.11"},{"v":0.128988424,"d":"0.13"}]
["48187","Guadalupe","TX",{"v":1.1441306376317044,"d":"1.14"},{"v":1.1441306376317044,"d":"1.14"},{"v":0.07953644,"d":"0.08"}]
["48189","Hale","TX",{"v":1.17025301914542,"d":"1.17"},{"v":1.17025301914542,"d":"1.17"},{"v":0.067409145,"d":"0.07"}]
["48191","Hall","TX",{"v":1.1068749801497217,"d":"1.11"},{"v":1.106874980149722,"d":"1.11"},{"v":0.078645311,"d":"0.08"}]
["48193","Hamilton","TX",{"v":1.1688975221916973,"d":"1.17"},{"v":1.168897522191697,"d":"1.17"},{"v":0.095574979,"d":"0.10"}]
["48195","Hansford","TX",{"v":1.1623817061922426,"d":"1.16"},{"v":1.1623817061922426,"d":"1.16"},{"v":0.073306357,"d":"0.07"}]
["48197","Hardeman","TX",{"v":1.1285607420610124,"d":"1.13"},{"v":1.1285607420610126,"d":"1.13"},{"v":0.085567989,"d":"0.09"}]
["48199","Hardin","TX",{"v":1.304797734975895,"d":"1.30"},{"v":1.3047977349758948,"d":"1.30"},{"v":0.18925914,"d":"0.19"}]
["48201","Harris","TX",{"v":0.016303783487865035,"d":"0.02"},{"v":0.016303783487865035,"d":"0.02"},{"v":0.198550209,"d":"0.20"}]
["48203","Harrison","TX",{"v":1.2060047652144197,"d":"1.21"},{"v":1.2060047652144197,"d":"1.21"},{"v":0.14546428,"d":"0.15"}]
["48205","Hartley","TX",{"v":1.2072143302852474,"d":"1.21"},{"v":1.2072143302852474,"d":"1.21"},{"v":0.075842786,"d":"0.08"}]
["48207","Haskell","TX",{"v":1.1686931185967442,"d":"1.17"},{"v":1.168693118596744,"d":"1.17"},{"v":0.077736643,"d":"0.08"}]
["48209","Hays","TX",{"v":1.1100017796559458,"d":"1.11"},{"v":1.1100017796559456,"d":"1.11"},{"v":0.09207234,"d":"0.09"}]
["48211","Hemphill","TX",{"v":1.1896486697602522,"d":"1.19"},{"v":1.189648669760252,"d":"1.19"},{"v":0.082643525,"d":"0.08"}]
["48213","Henderson","TX",{"v":1.3084674348297165,"d":"1.31"},{"v":1.3084674348297163,"d":"1.31"},{"v":0.128473491,"d":"0.13"}]
["48215","Hidalgo","TX",{"v":1.0738865694892772,"d":"1.07"},{"v":1.073886569489277,"d":"1.07"},{"v":0.055308143,"d":"0.06"}]
["48217","Hill","TX",{"v":1.2151653566603564,"d":"1.22"},{"v":1.2151653566603564,"d":"1.22"},{"v":0.10754724,"d":"0.11"}]
["48219","Hockley","TX",{"v":1.2005194891675017,"d":"1.20"},{"v":1.2005194891675017,"d":"1.20"},{"v":0.08064317799999998,"d":"0.08"}]
["48221","Hood","TX",{"v":1.2384613568816916,"d":"1.24"},{"v":1.2384613568816916,"d":"1.24"},{"v":0.10829930800000001,"d":"0.11"}]
["48223","Hopkins","TX",{"v":1.1792567830582565,"d":"1.18"},{"v":1.1792567830582568,"d":"1.18"},{"v":0.09993154,"d":"0.10"}]
["48225","Houston","TX",{"v":1.194177567648178,"d":"1.19"},{"v":1.194177567648178,"d":"1.19"},{"v":0.141404541,"d":"0.14"}]
["48227","Howard","TX",{"v":1.2015553251298259,"d":"1.20"},{"v":1.2015553251298259,"d":"1.20"},{"v":0.081671245,"d":"0.08"}]
["48229","Hudspeth","TX",{"v":1.2330920008348372,"d":"1.23"},{"v":1.233092000834837,"d":"1.23"},{"v":0.090244484,"d":"0.09"}]
["48231","Hunt","TX",{"v":1.2007569752898075,"d":"1.20"},{"v":1.2007569752898075,"d":"1.20"},{"v":0.106132755,"d":"0.11"}]
["48233","Hutchinson","TX",{"v":1.1778765780708669,"d":"1.18"},{"v":1.1778765780708667,"d":"1.18"},{"v":0.06815759400000002,"d":"0.07"}]
["48235","Irion","TX",{"v":1.203852989728672,"d":"1.20"},{"v":1.203852989728672,"d":"1.20"},{"v":0.098576694,"d":"0.10"}]
["48237","Jack","TX",{"v":1.180560653727882,"d":"1.18"},{"v":1.180560653727882,"d":"1.18"},{"v":0.100865608,"d":"0.10"}]
["48239","Jackson","TX",{"v":1.1318615898255702,"d":"1.13"},{"v":1.1318615898255702,"d":"1.13"},{"v":0.071060534,"d":"0.07"}]
["48241","Jasper","TX",{"v":1.2906525291577173,"d":"1.29"},{"v":1.2906525291577176,"d":"1.29"},{"v":0.20051593,"d":"0.20"}]
["48243","Jeff Davis","TX",{"v":1.1877357842140368,"d":"1.19"},{"v":1.1877357842140368,"d":"1.19"},{"v":0.089171474,"d":"0.09"}]
["48245","Jefferson","TX",{"v":1.1477521412996117,"d":"1.15"},{"v":1.147752141299612,"d":"1.15"},{"v":0.048139889,"d":"0.05"}]
["48247","Jim Hogg","TX",{"v":1.069972227754066,"d":"1.07"},{"v":1.069972227754066,"d":"1.07"},{"v":0.048039055,"d":"0.05"}]
["48249","Jim Wells","TX",{"v":1.0990026380375724,"d":"1.10"},{"v":1.0990026380375724,"d":"1.10"},{"v":0.061257755,"d":"0.06"}]
["48251","Johnson","TX",{"v":1.2103510298692652,"d":"1.21"},{"v":1.2103510298692655,"d":"1.21"},{"v":0.106110043,"d":"0.11"}]
["48253","Jones","TX",{"v":1.2099780131916316,"d":"1.21"},{"v":1.2099780131916316,"d":"1.21"},{"v":0.10081977,"d":"0.10"}]
["48255","Karnes","TX",{"v":1.1184978961340424,"d":"1.12"},{"v":1.1184978961340424,"d":"1.12"},{"v":0.068941807,"d":"0.07"}]
["48257","Kaufman","TX",{"v":1.1955756817425063,"d":"1.20"},{"v":1.1955756817425065,"d":"1.20"},{"v":0.100241049,"d":"0.10"}]
["48259","Kendall","TX",{"v":1.1936772278220218,"d":"1.19"},{"v":1.1936772278220218,"d":"1.19"},{"v":0.121376575,"d":"0.12"}]
["48261","Kenedy","TX",{"v":1.1360024811692515,"d":"1.14"},{"v":1.1360024811692515,"d":"1.14"},{"v":0.072412292,"d":"0.07"}]
["48263","Kent","TX",{"v":1.26722038263477,"d":"1.27"},{"v":1.2672203826347703,"d":"1.27"},{"v":0.138956813,"d":"0.14"}]
["48265","Kerr","TX",{"v":1.1979424961775824,"d":"1.20"},{"v":1.1979424961775824,"d":"1.20"},{"v":0.115152815,"d":"0.12"}]
["48267","Kimble","TX",{"v":1.1787125151370743,"d":"1.18"},{"v":1.1787125151370743,"d":"1.18"},{"v":0.099401304,"d":"0.10"}]
["48269","King","TX",{"v":1.2579358178105748,"d":"1.26"},{"v":1.257935817810575,"d":"1.26"},{"v":0.133505832,"d":"0.13"}]
["48271","Kinney","TX",{"v":1.1951301491969677,"d":"1.20"},{"v":1.1951301491969677,"d":"1.20"},{"v":0.07106562,"d":"0.07"}]
["48273","Kleberg","TX",{"v":1.1089374944250368,"d":"1.11"},{"v":1.108937494425037,"d":"1.11"},{"v":0.048559308,"d":"0.05"}]
["48275","Knox","TX",{"v":1.118985411114077,"d":"1.12"},{"v":1.1189854111140767,"d":"1.12"},{"v":0.090368339,"d":"0.09"}]
["48277","Lamar","TX",{"v":1.1776189628536722,"d":"1.18"},{"v":1.1776189628536724,"d":"1.18"},{"v":0.10174594600000002,"d":"0.10"}]
["48279","Lamb","TX",{"v":1.1845674147039116,"d":"1.18"},{"v":1.1845674147039116,"d":"1.18"},{"v":0.081191431,"d":"0.08"}]
["48281","Lampasas","TX",{"v":1.178073482178221,"d":"1.18"},{"v":1.178073482178221,"d":"1.18"},{"v":0.09916397,"d":"0.10"}]
["48283","La Salle","TX",{"v":1.134075963647338,"d":"1.13"},{"v":1.134075963647338,"d":"1.13"},{"v":0.06147202100000001,"d":"0.06"}]
["48285","Lavaca","TX",{"v":1.1316302569149852,"d":"1.13"},{"v":1.131630256914985,"d":"1.13"},{"v":0.090641071,"d":"0.09"}]
["48287","Lee","TX",{"v":1.156780760413257,"d":"1.16"},{"v":1.156780760413257,"d":"1.16"},{"v":0.087835391,"d":"0.09"}]
["48289","Leon","TX",{"v":1.3334554099755742,"d":"1.33"},{"v":1.3334554099755744,"d":"1.33"},{"v":0.152914919,"d":"0.15"}]
["48291","Liberty","TX",{"v":1.1665405376413447,"d":"1.17"},{"v":1.1665405376413447,"d":"1.17"},{"v":0.12276751200000001,"d":"0.12"}]
["48293","Limestone","TX",{"v":1.203663258253071,"d":"1.20"},{"v":1.203663258253071,"d":"1.20"},{"v":0.101933261,"d":"0.10"}]
["48295","Lipscomb","TX",{"v":1.1878136483643404,"d":"1.19"},{"v":1.1878136483643407,"d":"1.19"},{"v":0.090635437,"d":"0.09"}]
["48297","Live Oak","TX",{"v":1.1490348385457418,"d":"1.15"},{"v":1.1490348385457418,"d":"1.15"},{"v":0.087164626,"d":"0.09"}]
["48299","Llano","TX",{"v":1.1999547018679788,"d":"1.20"},{"v":1.1999547018679788,"d":"1.20"},{"v":0.107469542,"d":"0.11"}]
["48301","Loving","TX",{"v":1.2786433463882343,"d":"1.28"},{"v":1.2786433463882343,"d":"1.28"},{"v":0.09857959,"d":"0.10"}]
["48303","Lubbock","TX",{"v":1.1714085137143464,"d":"1.17"},{"v":1.1714085137143464,"d":"1.17"},{"v":0.080045167,"d":"0.08"}]
["48305","Lynn","TX",{"v":1.212221467912505,"d":"1.21"},{"v":1.212221467912505,"d":"1.21"},{"v":0.088949087,"d":"0.09"}]
["48307","McCulloch","TX",{"v":1.1218854403038914,"d":"1.12"},{"v":1.1218854403038914,"d":"1.12"},{"v":0.076546652,"d":"0.08"}]
["48309","McLennan","TX",{"v":1.148555385263162,"d":"1.15"},{"v":1.1485553852631618,"d":"1.15"},{"v":0.08750206,"d":"0.09"}]
["48311","McMullen","TX",{"v":1.1287425393779673,"d":"1.13"},{"v":1.1287425393779675,"d":"1.13"},{"v":0.07930381,"d":"0.08"}]
["48313","Madison","TX",{"v":1.179101928262471,"d":"1.18"},{"v":1.179101928262471,"d":"1.18"},{"v":0.105673857,"d":"0.11"}]
["48315","Marion","TX",{"v":1.231185158452036,"d":"1.23"},{"v":1.231185158452036,"d":"1.23"},{"v":0.187791482,"d":"0.19"}]
["48317","Martin","TX",{"v":1.25251846263352,"d":"1.25"},{"v":1.25251846263352,"d":"1.25"},{"v":0.11358612700000001,"d":"0.11"}]
["48319","Mason","TX",{"v":1.212317834348552,"d":"1.21"},{"v":1.212317834348552,"d":"1.21"},{"v":0.128126944,"d":"0.13"}]
["48321","Matagorda","TX",{"v":1.1236054258670114,"d":"1.12"},{"v":1.1236054258670116,"d":"1.12"},{"v":0.056499431,"d":"0.06"}]
["48323","Maverick","TX",{"v":1.1001007034200738,"d":"1.10"},{"v":1.1001007034200736,"d":"1.10"},{"v":0.043479121,"d":"0.04"}]
["48325","Medina","TX",{"v":1.1737590326073164,"d":"1.17"},{"v":1.1737590326073164,"d":"1.17"},{"v":0.093976168,"d":"0.09"}]
["48327","Menard","TX",{"v":1.2023189095477513,"d":"1.20"},{"v":1.2023189095477513,"d":"1.20"},{"v":0.110248976,"d":"0.11"}]
["48329","Midland","TX",{"v":1.2112285385206132,"d":"1.21"},{"v":1.2112285385206134,"d":"1.21"},{"v":0.080505968,"d":"0.08"}]
["48331","Milam","TX",{"v":1.1900275203855795,"d":"1.19"},{"v":1.1900275203855797,"d":"1.19"},{"v":0.103321926,"d":"0.10"}]
["48333","Mills","TX",{"v":1.189754833483437,"d":"1.19"},{"v":1.1897548334834367,"d":"1.19"},{"v":0.11694302699999999,"d":"0.12"}]
["48335","Mitchell","TX",{"v":1.191023906872277,"d":"1.19"},{"v":1.1910239068722772,"d":"1.19"},{"v":0.08376578799999998,"d":"0.08"}]
["48337","Montague","TX",{"v":1.1761689849795023,"d":"1.18"},{"v":1.1761689849795023,"d":"1.18"},{"v":0.095531808,"d":"0.10"}]
["48339","Montgomery","TX",{"v":1.105936383723405,"d":"1.11"},{"v":1.1059363837234053,"d":"1.11"},{"v":0.138659557,"d":"0.14"}]
["48341","Moore","TX",{"v":1.192879432791263,"d":"1.19"},{"v":1.192879432791263,"d":"1.19"},{"v":0.066788498,"d":"0.07"}]
["48343","Morris","TX",{"v":1.2091105585484354,"d":"1.21"},{"v":1.2091105585484356,"d":"1.21"},{"v":0.136875523,"d":"0.14"}]
["48345","Motley","TX",{"v":1.2566810824467252,"d":"1.26"},{"v":1.256681082446725,"d":"1.26"},{"v":0.12387832,"d":"0.12"}]
["48347","Nacogdoches","TX",{"v":1.1785474966311447,"d":"1.18"},{"v":1.1785474966311447,"d":"1.18"},{"v":0.146519937,"d":"0.15"}]
["48349","Navarro","TX",{"v":1.1762855072766216,"d":"1.18"},{"v":1.1762855072766216,"d":"1.18"},{"v":0.092121469,"d":"0.09"}]
["48351","Newton","TX",{"v":1.2855338409023789,"d":"1.29"},{"v":1.2855338409023787,"d":"1.29"},{"v":0.227207506,"d":"0.23"}]
["48353","Nolan","TX",{"v":1.158843718402324,"d":"1.16"},{"v":1.1588437184023241,"d":"1.16"},{"v":0.091661256,"d":"0.09"}]
["48355","Nueces","TX",{"v":1.0790779193310658,"d":"1.08"},{"v":1.0790779193310658,"d":"1.08"},{"v":0.053156389000000005,"d":"0.05"}]
["48357","Ochiltree","TX",{"v":1.1649915945976417,"d":"1.16"},{"v":1.1649915945976417,"d":"1.16"},{"v":0.060983789,"d":"0.06"}]
["48359","Oldham","TX",{"v":1.1698110888712832,"d":"1.17"},{"v":1.169811088871283,"d":"1.17"},{"v":0.09863412,"d":"0.10"}]
["48361","Orange","TX",{"v":1.1529171124345963,"d":"1.15"},{"v":1.1529171124345963,"d":"1.15"},{"v":0.093928394,"d":"0.09"}]
["48363","Palo Pinto","TX",{"v":1.1816484044543631,"d":"1.18"},{"v":1.1816484044543631,"d":"1.18"},{"v":0.11069094900000001,"d":"0.11"}]
["48365","Panola","TX",{"v":1.2656065828935612,"d":"1.27"},{"v":1.265606582893561,"d":"1.27"},{"v":0.157270633,"d":"0.16"}]
["48367","Parker","TX",{"v":1.222428231870681,"d":"1.22"},{"v":1.222428231870681,"d":"1.22"},{"v":0.118898826,"d":"0.12"}]
["48369","Parmer","TX",{"v":1.2004777729683314,"d":"1.20"},{"v":1.2004777729683314,"d":"1.20"},{"v":0.083748794,"d":"0.08"}]
["48371","Pecos","TX",{"v":1.166314775437618,"d":"1.17"},{"v":1.1663147754376177,"d":"1.17"},{"v":0.067840362,"d":"0.07"}]
["48373","Polk","TX",{"v":1.2249882306524604,"d":"1.22"},{"v":1.2249882306524604,"d":"1.22"},{"v":0.20218383099999998,"d":"0.20"}]
["48375","Potter","TX",{"v":1.157641048924376,"d":"1.16"},{"v":1.1576410489243762,"d":"1.16"},{"v":0.064920528,"d":"0.06"}]
["48377","Presidio","TX",{"v":1.1904663137265825,"d":"1.19"},{"v":1.1904663137265825,"d":"1.19"},{"v":0.075601785,"d":"0.08"}]
["48379","Rains","TX",{"v":1.2289327943507622,"d":"1.23"},{"v":1.228932794350762,"d":"1.23"},{"v":0.126601507,"d":"0.13"}]
["48381","Randall","TX",{"v":1.1844352491471883,"d":"1.18"},{"v":1.1844352491471886,"d":"1.18"},{"v":0.068599109,"d":"0.07"}]
["48383","Reagan","TX",{"v":1.1424107980297447,"d":"1.14"},{"v":1.1424107980297449,"d":"1.14"},{"v":0.053646539,"d":"0.05"}]
["48385","Real","TX",{"v":1.251239655570859,"d":"1.25"},{"v":1.251239655570859,"d":"1.25"},{"v":0.16586514,"d":"0.17"}]
["48387","Red River","TX",{"v":1.2836184877754477,"d":"1.28"},{"v":1.2836184877754475,"d":"1.28"},{"v":0.126822324,"d":"0.13"}]
["48389","Reeves","TX",{"v":1.08511083309335,"d":"1.09"},{"v":1.0851108330933503,"d":"1.09"},{"v":0.046441231,"d":"0.05"}]
["48391","Refugio","TX",{"v":1.1018099174815101,"d":"1.10"},{"v":1.1018099174815101,"d":"1.10"},{"v":0.066865072,"d":"0.07"}]
["48393","Roberts","TX",{"v":1.226168932734541,"d":"1.23"},{"v":1.226168932734541,"d":"1.23"},{"v":0.10929586,"d":"0.11"}]
["48395","Robertson","TX",{"v":1.1750910550351266,"d":"1.18"},{"v":1.1750910550351268,"d":"1.18"},{"v":0.110045742,"d":"0.11"}]
["48397","Rockwall","TX",{"v":1.074641507240521,"d":"1.07"},{"v":1.0746415072405209,"d":"1.07"},{"v":0.091896405,"d":"0.09"}]
["48399","Runnels","TX",{"v":1.15443718147516,"d":"1.15"},{"v":1.15443718147516,"d":"1.15"},{"v":0.077256484,"d":"0.08"}]
["48401","Rusk","TX",{"v":1.2630280924310298,"d":"1.26"},{"v":1.2630280924310295,"d":"1.26"},{"v":0.141790839,"d":"0.14"}]
["48403","Sabine","TX",{"v":1.3079634738200896,"d":"1.31"},{"v":1.3079634738200896,"d":"1.31"},{"v":0.188062934,"d":"0.19"}]
["48405","San Augustine","TX",{"v":1.2478606744739562,"d":"1.25"},{"v":1.2478606744739562,"d":"1.25"},{"v":0.182778996,"d":"0.18"}]
["48407","San Jacinto","TX",{"v":1.2624060259060514,"d":"1.26"},{"v":1.2624060259060517,"d":"1.26"},{"v":0.206002649,"d":"0.21"}]
["48409","San Patricio","TX",{"v":1.1005212070125248,"d":"1.10"},{"v":1.1005212070125248,"d":"1.10"},{"v":0.04969691400000001,"d":"0.05"}]
["48411","San Saba","TX",{"v":1.1658916527483707,"d":"1.17"},{"v":1.1658916527483707,"d":"1.17"},{"v":0.10089714400000001,"d":"0.10"}]
["48413","Schleicher","TX",{"v":1.1705306711495707,"d":"1.17"},{"v":1.1705306711495709,"d":"1.17"},{"v":0.091254414,"d":"0.09"}]
["48415","Scurry","TX",{"v":1.1703287932379853,"d":"1.17"},{"v":1.1703287932379853,"d":"1.17"},{"v":0.07301120999999999,"d":"0.07"}]
["48417","Shackelford","TX",{"v":1.1766497147491226,"d":"1.18"},{"v":1.1766497147491224,"d":"1.18"},{"v":0.085544746,"d":"0.09"}]
["48419","Shelby","TX",{"v":1.2176389220832413,"d":"1.22"},{"v":1.217638922083241,"d":"1.22"},{"v":0.174278749,"d":"0.17"}]
["48421","Sherman","TX",{"v":1.1906586248118887,"d":"1.19"},{"v":1.1906586248118887,"d":"1.19"},{"v":0.088737964,"d":"0.09"}]
["48423","Smith","TX",{"v":1.163951359935076,"d":"1.16"},{"v":1.163951359935076,"d":"1.16"},{"v":0.122242151,"d":"0.12"}]
["48425","Somervell","TX",{"v":1.2358368843465268,"d":"1.24"},{"v":1.235836884346527,"d":"1.24"},{"v":0.145605124,"d":"0.15"}]
["48427","Starr","TX",{"v":1.119785254800493,"d":"1.12"},{"v":1.119785254800493,"d":"1.12"},{"v":0.054589524,"d":"0.05"}]
["48429","Stephens","TX",{"v":1.181609482748487,"d":"1.18"},{"v":1.181609482748487,"d":"1.18"},{"v":0.086153312,"d":"0.09"}]
["48431","Sterling","TX",{"v":1.1879278386362409,"d":"1.19"},{"v":1.1879278386362409,"d":"1.19"},{"v":0.087647145,"d":"0.09"}]
["48433","Stonewall","TX",{"v":1.2533738610948557,"d":"1.25"},{"v":1.2533738610948557,"d":"1.25"},{"v":0.141107593,"d":"0.14"}]
["48435","Sutton","TX",{"v":1.1613889466158374,"d":"1.16"},{"v":1.1613889466158371,"d":"1.16"},{"v":0.068368479,"d":"0.07"}]
["48437","Swisher","TX",{"v":1.1652192794693361,"d":"1.17"},{"v":1.1652192794693361,"d":"1.17"},{"v":0.072318683,"d":"0.07"}]
["48439","Tarrant","TX",{"v":0.054961762126278194,"d":"0.05"},{"v":0.05496176212627819,"d":"0.05"},{"v":0.215356667,"d":"0.22"}]
["48441","Taylor","TX",{"v":1.163619141487123,"d":"1.16"},{"v":1.1636191414871229,"d":"1.16"},{"v":0.088555362,"d":"0.09"}]
["48443","Terrell","TX",{"v":1.1970633970380258,"d":"1.20"},{"v":1.1970633970380258,"d":"1.20"},{"v":0.098609297,"d":"0.10"}]
["48445","Terry","TX",{"v":1.1766778672924751,"d":"1.18"},{"v":1.1766778672924751,"d":"1.18"},{"v":0.068820835,"d":"0.07"}]
["48447","Throckmorton","TX",{"v":1.168357936303799,"d":"1.17"},{"v":1.168357936303799,"d":"1.17"},{"v":0.092208674,"d":"0.09"}]
["48449","Titus","TX",{"v":1.269270125908191,"d":"1.27"},{"v":1.269270125908191,"d":"1.27"},{"v":0.11426143399999998,"d":"0.11"}]
["48451","Tom Green","TX",{"v":1.1525800266820043,"d":"1.15"},{"v":1.152580026682004,"d":"1.15"},{"v":0.064514182,"d":"0.06"}]
["48453","Travis","TX",{"v":0.6628337280580111,"d":"0.66"},{"v":0.6628337280580112,"d":"0.66"},{"v":0.103652851,"d":"0.10"}]
["48455","Trinity","TX",{"v":1.2849420086938583,"d":"1.28"},{"v":1.2849420086938583,"d":"1.28"},{"v":0.191465978,"d":"0.19"}]
["48457","Tyler","TX",{"v":1.2775771193795014,"d":"1.28"},{"v":1.2775771193795011,"d":"1.28"},{"v":0.224456382,"d":"0.22"}]
["48459","Upshur","TX",{"v":1.3165445292457336,"d":"1.32"},{"v":1.3165445292457334,"d":"1.32"},{"v":0.15633765,"d":"0.16"}]
["48461","Upton","TX",{"v":1.1543447438364536,"d":"1.15"},{"v":1.1543447438364538,"d":"1.15"},{"v":0.074354588,"d":"0.07"}]
["48463","Uvalde","TX",{"v":1.1845338056421504,"d":"1.18"},{"v":1.1845338056421504,"d":"1.18"},{"v":0.087924916,"d":"0.09"}]
["48465","Val Verde","TX",{"v":1.15972680900249,"d":"1.16"},{"v":1.15972680900249,"d":"1.16"},{"v":0.064099462,"d":"0.06"}]
["48467","Van Zandt","TX",{"v":1.311391230775422,"d":"1.31"},{"v":1.311391230775422,"d":"1.31"},{"v":0.117677968,"d":"0.12"}]
["48469","Victoria","TX",{"v":1.0967042228301482,"d":"1.10"},{"v":1.0967042228301482,"d":"1.10"},{"v":0.061987419,"d":"0.06"}]
["48471","Walker","TX",{"v":1.1890574102220355,"d":"1.19"},{"v":1.1890574102220355,"d":"1.19"},{"v":0.158633616,"d":"0.16"}]
["48473","Waller","TX",{"v":1.1990322721232562,"d":"1.20"},{"v":1.1990322721232565,"d":"1.20"},{"v":0.107958683,"d":"0.11"}]
["48475","Ward","TX",{"v":1.1212121229098864,"d":"1.12"},{"v":1.1212121229098866,"d":"1.12"},{"v":0.054857723,"d":"0.05"}]
["48477","Washington","TX",{"v":1.1248363115002353,"d":"1.12"},{"v":1.1248363115002353,"d":"1.12"},{"v":0.077866886,"d":"0.08"}]
["48479","Webb","TX",{"v":1.1141161499445424,"d":"1.11"},{"v":1.1141161499445427,"d":"1.11"},{"v":0.043248339,"d":"0.04"}]
["48481","Wharton","TX",{"v":1.1062798234824125,"d":"1.11"},{"v":1.1062798234824123,"d":"1.11"},{"v":0.062638231,"d":"0.06"}]
["48483","Wheeler","TX",{"v":1.1571565261994112,"d":"1.16"},{"v":1.1571565261994115,"d":"1.16"},{"v":0.083784314,"d":"0.08"}]
["48485","Wichita","TX",{"v":1.146149054413653,"d":"1.15"},{"v":1.146149054413653,"d":"1.15"},{"v":0.063856757,"d":"0.06"}]
["48487","Wilbarger","TX",{"v":1.1237783929557195,"d":"1.12"},{"v":1.1237783929557195,"d":"1.12"},{"v":0.06186522299999999,"d":"0.06"}]
["48489","Willacy","TX",{"v":1.0862709750651145,"d":"1.09"},{"v":1.0862709750651143,"d":"1.09"},{"v":0.049077164,"d":"0.05"}]
["48491","Williamson","TX",{"v":1.104557356932299,"d":"1.10"},{"v":1.104557356932299,"d":"1.10"},{"v":0.080790569,"d":"0.08"}]
["48493","Wilson","TX",{"v":1.169680298585426,"d":"1.17"},{"v":1.1696802985854262,"d":"1.17"},{"v":0.090428074,"d":"0.09"}]
["48495","Winkler","TX",{"v":1.0918013248790903,"d":"1.09"},{"v":1.0918013248790905,"d":"1.09"},{"v":0.044760617,"d":"0.04"}]
["48497","Wise","TX",{"v":1.2374515912957935,"d":"1.24"},{"v":1.2374515912957935,"d":"1.24"},{"v":0.11529122900000001,"d":"0.12"}]
["48499","Wood","TX",{"v":1.2839663994745603,"d":"1.28"},{"v":1.28396639947456,"d":"1.28"},{"v":0.146765149,"d":"0.15"}]
["48501","Yoakum","TX",{"v":1.2162723703938603,"d":"1.22"},{"v":1.21627237039386,"d":"1.22"},{"v":0.08418032,"d":"0.08"}]
["48503","Young","TX",{"v":1.1609759382106644,"d":"1.16"},{"v":1.1609759382106644,"d":"1.16"},{"v":0.07761006,"d":"0.08"}]
["48505","Zapata","TX",{"v":1.1578834925248496,"d":"1.16"},{"v":1.1578834925248493,"d":"1.16"},{"v":0.054359304,"d":"0.05"}]
["48507","Zavala","TX",{"v":1.1059599766770598,"d":"1.11"},{"v":1.1059599766770594,"d":"1.11"},{"v":0.060783839,"d":"0.06"}]
["49001","Beaver","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.11088065799999999,"d":"0.11"}]
["49003","Box Elder","UT",{"v":0.6535072931066191,"d":"0.65"},{"v":0.6535072931066191,"d":"0.65"},{"v":0.072200791,"d":"0.07"}]
["49005","Cache","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.095591828,"d":"0.10"}]
["49007","Carbon","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.07787204,"d":"0.08"}]
["49009","Daggett","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.39231429600000006,"d":"0.39"}]
["49011","Davis","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.127983831,"d":"0.13"}]
["49013","Duchesne","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.171602695,"d":"0.17"}]
["49015","Emery","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.089565078,"d":"0.09"}]
["49017","Garfield","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.18922986899999997,"d":"0.19"}]
["49019","Grand","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.07454651,"d":"0.07"}]
["49021","Iron","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.091166332,"d":"0.09"}]
["49023","Juab","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.089445204,"d":"0.09"}]
["49025","Kane","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.177230562,"d":"0.18"}]
["49027","Millard","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.097874263,"d":"0.10"}]
["49029","Morgan","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.210360126,"d":"0.21"}]
["49031","Piute","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.162551537,"d":"0.16"}]
["49033","Rich","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.266668776,"d":"0.27"}]
["49035","Salt Lake","UT",{"v":0.34636490078035154,"d":"0.35"},{"v":0.3463649007803515,"d":"0.35"},{"v":0.176456335,"d":"0.18"}]
["49037","San Juan","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.11367951700000001,"d":"0.11"}]
["49039","Sanpete","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.1247204,"d":"0.12"}]
["49041","Sevier","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.134960207,"d":"0.13"}]
["49043","Summit","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.20393297,"d":"0.20"}]
["49045","Tooele","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.066002947,"d":"0.07"}]
["49047","Uintah","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.124738918,"d":"0.12"}]
["49049","Utah","UT",{"v":0.6692064889852118,"d":"0.67"},{"v":0.6692064889852118,"d":"0.67"},{"v":0.097035049,"d":"0.10"}]
["49051","Wasatch","UT",{"v":0.7867968935596765,"d":"0.79"},{"v":0.7867968935596765,"d":"0.79"},{"v":0.198398685,"d":"0.20"}]
["49053","Washington","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.047969073,"d":"0.05"}]
["49055","Wayne","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.138895853,"d":"0.14"}]
["49057","Weber","UT",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.168694955,"d":"0.17"}]
["50001","Addison","VT",{"v":8.00727528930179,"d":"8.01"},{"v":8.00727528930179,"d":"8.01"},{"v":3.667571611,"d":"3.67"}]
["50003","Bennington","VT",{"v":7.793554710791102,"d":"7.79"},{"v":7.793554710791103,"d":"7.79"},{"v":4.887470405,"d":"4.89"}]
["50005","Caledonia","VT",{"v":7.7955766275976695,"d":"7.80"},{"v":7.79557662759767,"d":"7.80"},{"v":5.354684087,"d":"5.35"}]
["50007","Chittenden","VT",{"v":7.2091873812507234,"d":"7.21"},{"v":7.209187381250724,"d":"7.21"},{"v":2.350688377,"d":"2.35"}]
["50009","Essex","VT",{"v":7.740959293562762,"d":"7.74"},{"v":7.740959293562762,"d":"7.74"},{"v":5.993513808,"d":"5.99"}]
["50011","Franklin","VT",{"v":7.409257424986285,"d":"7.41"},{"v":7.4092574249862855,"d":"7.41"},{"v":2.9946062,"d":"2.99"}]
["50013","Grand Isle","VT",{"v":7.329034181278662,"d":"7.33"},{"v":7.3290341812786615,"d":"7.33"},{"v":2.372158348,"d":"2.37"}]
["50015","Lamoille","VT",{"v":8.102942961453634,"d":"8.10"},{"v":8.102942961453634,"d":"8.10"},{"v":6.129672101,"d":"6.13"}]
["50017","Orange","VT",{"v":8.351914536867717,"d":"8.35"},{"v":8.351914536867717,"d":"8.35"},{"v":5.783681168,"d":"5.78"}]
["50019","Orleans","VT",{"v":7.876616311390892,"d":"7.88"},{"v":7.876616311390891,"d":"7.88"},{"v":5.037964546,"d":"5.04"}]
["50021","Rutland","VT",{"v":7.824775370068389,"d":"7.82"},{"v":7.824775370068391,"d":"7.82"},{"v":4.33941784,"d":"4.34"}]
["50023","Washington","VT",{"v":8.123420931319865,"d":"8.12"},{"v":8.123420931319867,"d":"8.12"},{"v":5.32926835,"d":"5.33"}]
["50025","Windham","VT",{"v":7.959653230330469,"d":"7.96"},{"v":7.959653230330469,"d":"7.96"},{"v":4.673890279,"d":"4.67"}]
["50027","Windsor","VT",{"v":7.794813641925546,"d":"7.79"},{"v":7.794813641925546,"d":"7.79"},{"v":4.542973824,"d":"4.54"}]
["51001","Accomack","VA",{"v":2.5487114488650384,"d":"2.55"},{"v":2.5487114488650384,"d":"2.55"},{"v":0.366107025,"d":"0.37"}]
["51003","Albemarle","VA",{"v":2.5077205828839864,"d":"2.51"},{"v":2.5077205828839864,"d":"2.51"},{"v":0.656025216,"d":"0.66"}]
["51005","Alleghany","VA",{"v":2.8772212311329715,"d":"2.88"},{"v":2.877221231132971,"d":"2.88"},{"v":0.950937494,"d":"0.95"}]
["51007","Amelia","VA",{"v":2.8405640832512757,"d":"2.84"},{"v":2.840564083251276,"d":"2.84"},{"v":0.731108451,"d":"0.73"}]
["51009","Amherst","VA",{"v":2.8334820597656245,"d":"2.83"},{"v":2.833482059765624,"d":"2.83"},{"v":0.811624948,"d":"0.81"}]
["51011","Appomattox","VA",{"v":3.0131905347467125,"d":"3.01"},{"v":3.0131905347467125,"d":"3.01"},{"v":0.759474754,"d":"0.76"}]
["51013","Arlington","VA",{"v":2.4505980472451482E-15,"d":"0.00"},{"v":2.4505980472451482E-15,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["51015","Augusta","VA",{"v":3.0996198470469785,"d":"3.10"},{"v":3.0996198470469785,"d":"3.10"},{"v":0.773097635,"d":"0.77"}]
["51017","Bath","VA",{"v":3.031821262558483,"d":"3.03"},{"v":3.0318212625584824,"d":"3.03"},{"v":1.206582576,"d":"1.21"}]
["51019","Bedford","VA",{"v":2.6844604756032346,"d":"2.68"},{"v":2.6844604756032346,"d":"2.68"},{"v":0.707269619,"d":"0.71"}]
["51021","Bland","VA",{"v":2.729419118249247,"d":"2.73"},{"v":2.7294191182492464,"d":"2.73"},{"v":1.019907812,"d":"1.02"}]
["51023","Botetourt","VA",{"v":2.7610013154229147,"d":"2.76"},{"v":2.7610013154229143,"d":"2.76"},{"v":0.843966889,"d":"0.84"}]
["51025","Brunswick","VA",{"v":2.6429988921147656,"d":"2.64"},{"v":2.6429988921147656,"d":"2.64"},{"v":0.7388815260000001,"d":"0.74"}]
["51027","Buchanan","VA",{"v":2.8698852483216704,"d":"2.87"},{"v":2.8698852483216704,"d":"2.87"},{"v":1.153184778,"d":"1.15"}]
["51029","Buckingham","VA",{"v":2.860405339885339,"d":"2.86"},{"v":2.8604053398853386,"d":"2.86"},{"v":0.7796253699999999,"d":"0.78"}]
["51031","Campbell","VA",{"v":2.8666137279341606,"d":"2.87"},{"v":2.8666137279341606,"d":"2.87"},{"v":0.651192796,"d":"0.65"}]
["51033","Caroline","VA",{"v":2.860769804895244,"d":"2.86"},{"v":2.8607698048952437,"d":"2.86"},{"v":0.694026155,"d":"0.69"}]
["51035","Carroll","VA",{"v":3.1195685593895983,"d":"3.12"},{"v":3.1195685593895988,"d":"3.12"},{"v":0.888134064,"d":"0.89"}]
["51036","Charles City","VA",{"v":2.707404060538754,"d":"2.71"},{"v":2.7074040605387544,"d":"2.71"},{"v":0.58918067,"d":"0.59"}]
["51037","Charlotte","VA",{"v":2.4009888442366614,"d":"2.40"},{"v":2.4009888442366614,"d":"2.40"},{"v":0.76858174,"d":"0.77"}]
["51041","Chesterfield","VA",{"v":2.436867549605924,"d":"2.44"},{"v":2.436867549605924,"d":"2.44"},{"v":0.599382552,"d":"0.60"}]
["51043","Clarke","VA",{"v":2.565150524298706,"d":"2.57"},{"v":2.5651505242987054,"d":"2.57"},{"v":0.561418748,"d":"0.56"}]
["51045","Craig","VA",{"v":3.2145119552932155,"d":"3.21"},{"v":3.2145119552932155,"d":"3.21"},{"v":1.15569572,"d":"1.16"}]
["51047","Culpeper","VA",{"v":2.6989537823024454,"d":"2.70"},{"v":2.6989537823024454,"d":"2.70"},{"v":0.540770222,"d":"0.54"}]
["51049","Cumberland","VA",{"v":2.5708907124370066,"d":"2.57"},{"v":2.5708907124370066,"d":"2.57"},{"v":0.730826256,"d":"0.73"}]
["51051","Dickenson","VA",{"v":3.0629778482944348,"d":"3.06"},{"v":3.0629778482944343,"d":"3.06"},{"v":1.096434543,"d":"1.10"}]
["51053","Dinwiddie","VA",{"v":2.761185029794424,"d":"2.76"},{"v":2.7611850297944245,"d":"2.76"},{"v":0.670266676,"d":"0.67"}]
["51057","Essex","VA",{"v":2.6533130036286616,"d":"2.65"},{"v":2.6533130036286616,"d":"2.65"},{"v":0.526023718,"d":"0.53"}]
["51059","Fairfax","VA",{"v":0.016306847088523736,"d":"0.02"},{"v":0.016306847088523736,"d":"0.02"},{"v":1.447190847,"d":"1.45"}]
["51061","Fauquier","VA",{"v":2.9578914870504724,"d":"2.96"},{"v":2.9578914870504724,"d":"2.96"},{"v":0.574764633,"d":"0.57"}]
["51063","Floyd","VA",{"v":2.6717425363498886,"d":"2.67"},{"v":2.6717425363498886,"d":"2.67"},{"v":0.907818977,"d":"0.91"}]
["51065","Fluvanna","VA",{"v":2.8209250320553947,"d":"2.82"},{"v":2.8209250320553947,"d":"2.82"},{"v":0.6899792770000001,"d":"0.69"}]
["51067","Franklin","VA",{"v":2.746219017364858,"d":"2.75"},{"v":2.7462190173648584,"d":"2.75"},{"v":0.706506397,"d":"0.71"}]
["51069","Frederick","VA",{"v":3.0559041219246352,"d":"3.06"},{"v":3.0559041219246352,"d":"3.06"},{"v":0.639520668,"d":"0.64"}]
["51071","Giles","VA",{"v":3.0274690070711814,"d":"3.03"},{"v":3.0274690070711814,"d":"3.03"},{"v":0.8894875029999999,"d":"0.89"}]
["51073","Gloucester","VA",{"v":2.4951792910295802,"d":"2.50"},{"v":2.4951792910295802,"d":"2.50"},{"v":0.499758529,"d":"0.50"}]
["51075","Goochland","VA",{"v":2.7201726390300327,"d":"2.72"},{"v":2.7201726390300327,"d":"2.72"},{"v":0.705964166,"d":"0.71"}]
["51077","Grayson","VA",{"v":2.971289749322814,"d":"2.97"},{"v":2.971289749322814,"d":"2.97"},{"v":0.9289945810000001,"d":"0.93"}]
["51079","Greene","VA",{"v":2.6353755988702283,"d":"2.64"},{"v":2.6353755988702283,"d":"2.64"},{"v":0.822849437,"d":"0.82"}]
["51081","Greensville","VA",{"v":2.766130508892402,"d":"2.77"},{"v":2.7661305088924024,"d":"2.77"},{"v":0.62679209,"d":"0.63"}]
["51083","Halifax","VA",{"v":2.617663391936494,"d":"2.62"},{"v":2.6176633919364947,"d":"2.62"},{"v":0.702215487,"d":"0.70"}]
["51085","Hanover","VA",{"v":2.385016866979929,"d":"2.39"},{"v":2.3850168669799294,"d":"2.39"},{"v":0.536459714,"d":"0.54"}]
["51087","Henrico","VA",{"v":1.0229634422198783,"d":"1.02"},{"v":1.0229634422198783,"d":"1.02"},{"v":0.631639499,"d":"0.63"}]
["51089","Henry","VA",{"v":2.4869653047632,"d":"2.49"},{"v":2.4869653047632,"d":"2.49"},{"v":0.738384319,"d":"0.74"}]
["51091","Highland","VA",{"v":3.042790289384792,"d":"3.04"},{"v":3.042790289384792,"d":"3.04"},{"v":1.060908672,"d":"1.06"}]
["51093","Isle of Wight","VA",{"v":2.4418062966350766,"d":"2.44"},{"v":2.4418062966350766,"d":"2.44"},{"v":0.392805743,"d":"0.39"}]
["51095","James City","VA",{"v":2.1948010711502177,"d":"2.19"},{"v":2.1948010711502177,"d":"2.19"},{"v":0.338988859,"d":"0.34"}]
["51097","King and Queen","VA",{"v":2.592851304207559,"d":"2.59"},{"v":2.5928513042075596,"d":"2.59"},{"v":0.637346492,"d":"0.64"}]
["51099","King George","VA",{"v":2.443588317495972,"d":"2.44"},{"v":2.4435883174959723,"d":"2.44"},{"v":0.489021686,"d":"0.49"}]
["51101","King William","VA",{"v":2.5610073515364014,"d":"2.56"},{"v":2.5610073515364014,"d":"2.56"},{"v":0.585436751,"d":"0.59"}]
["51103","Lancaster","VA",{"v":2.5365100886478853,"d":"2.54"},{"v":2.5365100886478853,"d":"2.54"},{"v":0.468308085,"d":"0.47"}]
["51105","Lee","VA",{"v":2.7033250262228554,"d":"2.70"},{"v":2.7033250262228554,"d":"2.70"},{"v":0.9525330609999999,"d":"0.95"}]
["51107","Loudoun","VA",{"v":2.579602949241288,"d":"2.58"},{"v":2.5796029492412877,"d":"2.58"},{"v":0.416544127,"d":"0.42"}]
["51109","Louisa","VA",{"v":2.9856023234813267,"d":"2.99"},{"v":2.9856023234813267,"d":"2.99"},{"v":0.729660603,"d":"0.73"}]
["51111","Lunenburg","VA",{"v":2.701527167497854,"d":"2.70"},{"v":2.701527167497854,"d":"2.70"},{"v":0.744151448,"d":"0.74"}]
["51113","Madison","VA",{"v":3.086873689911245,"d":"3.09"},{"v":3.0868736899112443,"d":"3.09"},{"v":0.811774082,"d":"0.81"}]
["51115","Mathews","VA",{"v":2.72832609364085,"d":"2.73"},{"v":2.72832609364085,"d":"2.73"},{"v":0.359852171,"d":"0.36"}]
["51117","Mecklenburg","VA",{"v":2.827419229901652,"d":"2.83"},{"v":2.827419229901652,"d":"2.83"},{"v":0.605949603,"d":"0.61"}]
["51119","Middlesex","VA",{"v":2.222138664614034,"d":"2.22"},{"v":2.2221386646140338,"d":"2.22"},{"v":0.480686423,"d":"0.48"}]
["51121","Montgomery","VA",{"v":3.027447650530143,"d":"3.03"},{"v":3.027447650530143,"d":"3.03"},{"v":0.710300433,"d":"0.71"}]
["51125","Nelson","VA",{"v":2.764594884801574,"d":"2.76"},{"v":2.764594884801574,"d":"2.76"},{"v":0.9071899649999999,"d":"0.91"}]
["51127","New Kent","VA",{"v":2.5783312308194177,"d":"2.58"},{"v":2.5783312308194177,"d":"2.58"},{"v":0.609891346,"d":"0.61"}]
["51131","Northampton","VA",{"v":2.576534120633512,"d":"2.58"},{"v":2.576534120633512,"d":"2.58"},{"v":0.324468629,"d":"0.32"}]
["51133","Northumberland","VA",{"v":2.688745997798945,"d":"2.69"},{"v":2.6887459977989456,"d":"2.69"},{"v":0.38885964,"d":"0.39"}]
["51135","Nottoway","VA",{"v":2.995104034416043,"d":"3.00"},{"v":2.9951040344160424,"d":"3.00"},{"v":0.642372042,"d":"0.64"}]
["51137","Orange","VA",{"v":2.906955312149392,"d":"2.91"},{"v":2.906955312149392,"d":"2.91"},{"v":0.685938061,"d":"0.69"}]
["51139","Page","VA",{"v":2.664203421739611,"d":"2.66"},{"v":2.664203421739611,"d":"2.66"},{"v":0.858858928,"d":"0.86"}]
["51141","Patrick","VA",{"v":2.5989703181651964,"d":"2.60"},{"v":2.5989703181651964,"d":"2.60"},{"v":0.866935738,"d":"0.87"}]
["51143","Pittsylvania","VA",{"v":2.6409500194636992,"d":"2.64"},{"v":2.6409500194636997,"d":"2.64"},{"v":0.665289863,"d":"0.67"}]
["51145","Powhatan","VA",{"v":2.8968439524632803,"d":"2.90"},{"v":2.8968439524632807,"d":"2.90"},{"v":0.758500306,"d":"0.76"}]
["51147","Prince Edward","VA",{"v":2.6862896091440835,"d":"2.69"},{"v":2.686289609144084,"d":"2.69"},{"v":0.671361678,"d":"0.67"}]
["51149","Prince George","VA",{"v":2.7578444425906805,"d":"2.76"},{"v":2.757844442590681,"d":"2.76"},{"v":0.562795761,"d":"0.56"}]
["51153","Prince William","VA",{"v":2.0171759875987885,"d":"2.02"},{"v":2.0171759875987885,"d":"2.02"},{"v":0.658816456,"d":"0.66"}]
["51155","Pulaski","VA",{"v":2.6271866603207052,"d":"2.63"},{"v":2.6271866603207052,"d":"2.63"},{"v":0.669554249,"d":"0.67"}]
["51157","Rappahannock","VA",{"v":3.093737699119572,"d":"3.09"},{"v":3.093737699119572,"d":"3.09"},{"v":0.873430587,"d":"0.87"}]
["51159","Richmond","VA",{"v":2.6651164311887996,"d":"2.67"},{"v":2.6651164311888,"d":"2.67"},{"v":0.51391788,"d":"0.51"}]
["51161","Roanoke","VA",{"v":2.7715280257567487,"d":"2.77"},{"v":2.7715280257567483,"d":"2.77"},{"v":0.705129128,"d":"0.71"}]
["51163","Rockbridge","VA",{"v":3.0338112181521875,"d":"3.03"},{"v":3.0338112181521875,"d":"3.03"},{"v":0.9464705309999999,"d":"0.95"}]
["51165","Rockingham","VA",{"v":3.100063684240514,"d":"3.10"},{"v":3.100063684240514,"d":"3.10"},{"v":0.785786307,"d":"0.79"}]
["51167","Russell","VA",{"v":3.214302043337377,"d":"3.21"},{"v":3.214302043337377,"d":"3.21"},{"v":0.858592529,"d":"0.86"}]
["51169","Scott","VA",{"v":2.7235590802981218,"d":"2.72"},{"v":2.7235590802981213,"d":"2.72"},{"v":0.8722819449999999,"d":"0.87"}]
["51171","Shenandoah","VA",{"v":3.2697247950930493,"d":"3.27"},{"v":3.2697247950930493,"d":"3.27"},{"v":0.72665611,"d":"0.73"}]
["51173","Smyth","VA",{"v":3.0369704359309146,"d":"3.04"},{"v":3.036970435930914,"d":"3.04"},{"v":0.84106354,"d":"0.84"}]
["51175","Southampton","VA",{"v":2.6541597263616334,"d":"2.65"},{"v":2.654159726361633,"d":"2.65"},{"v":0.570902245,"d":"0.57"}]
["51177","Spotsylvania","VA",{"v":2.4193137769688513,"d":"2.42"},{"v":2.4193137769688513,"d":"2.42"},{"v":0.550475974,"d":"0.55"}]
["51179","Stafford","VA",{"v":2.1407022145262165,"d":"2.14"},{"v":2.140702214526217,"d":"2.14"},{"v":0.475040404,"d":"0.48"}]
["51181","Surry","VA",{"v":2.7589031534972106,"d":"2.76"},{"v":2.7589031534972106,"d":"2.76"},{"v":0.530729883,"d":"0.53"}]
["51183","Sussex","VA",{"v":2.7072022519172116,"d":"2.71"},{"v":2.7072022519172125,"d":"2.71"},{"v":0.646637619,"d":"0.65"}]
["51185","Tazewell","VA",{"v":2.9621961167531716,"d":"2.96"},{"v":2.9621961167531716,"d":"2.96"},{"v":0.804356943,"d":"0.80"}]
["51187","Warren","VA",{"v":2.9831923365380493,"d":"2.98"},{"v":2.9831923365380493,"d":"2.98"},{"v":0.809891825,"d":"0.81"}]
["51191","Washington","VA",{"v":2.962253481425068,"d":"2.96"},{"v":2.9622534814250683,"d":"2.96"},{"v":0.7407384859999999,"d":"0.74"}]
["51193","Westmoreland","VA",{"v":2.659627362276272,"d":"2.66"},{"v":2.6596273622762725,"d":"2.66"},{"v":0.400596214,"d":"0.40"}]
["51195","Wise","VA",{"v":2.9470659673896775,"d":"2.95"},{"v":2.9470659673896775,"d":"2.95"},{"v":0.8934612920000001,"d":"0.89"}]
["51197","Wythe","VA",{"v":3.2328963678960636,"d":"3.23"},{"v":3.232896367896063,"d":"3.23"},{"v":0.702559899,"d":"0.70"}]
["51199","York","VA",{"v":2.796235380287913,"d":"2.80"},{"v":2.796235380287913,"d":"2.80"},{"v":0.266594443,"d":"0.27"}]
["51510","Alexandria City","VA",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["51520","Bristol City","VA",{"v":0.8772476343669496,"d":"0.88"},{"v":0.8772476343669496,"d":"0.88"},{"v":0.769503289,"d":"0.77"}]
["51530","Buena Vista City","VA",{"v":1.9899833322135019,"d":"1.99"},{"v":1.9899833322135017,"d":"1.99"},{"v":0.666574956,"d":"0.67"}]
["51540","Charlottesville City","VA",{"v":5.40420288371639e-06,"d":"0.00"},{"v":5.4042028837163911E-6,"d":"0.00"},{"v":4.311165203,"d":"4.31"}]
["51550","Chesapeake City","VA",{"v":2.1737892075806404,"d":"2.17"},{"v":2.1737892075806404,"d":"2.17"},{"v":0.400652803,"d":"0.40"}]
["51570","Colonial Heights City","VA",{"v":0.02931726904616504,"d":"0.03"},{"v":0.029317269046165037,"d":"0.03"},{"v":1.072532153,"d":"1.07"}]
["51580","Covington City","VA",{"v":1.6709164303368709,"d":"1.67"},{"v":1.6709164303368709,"d":"1.67"},{"v":0.885402594,"d":"0.89"}]
["51590","Danville City","VA",{"v":1.683730984821159,"d":"1.68"},{"v":1.683730984821159,"d":"1.68"},{"v":0.55011271,"d":"0.55"}]
["51595","Emporia City","VA",{"v":2.301064828423624,"d":"2.30"},{"v":2.301064828423624,"d":"2.30"},{"v":0.62810823,"d":"0.63"}]
["51600","Fairfax City","VA",{"v":4.6090338444656765E-4,"d":"0.00"},{"v":4.6090338444656755E-4,"d":"0.00"},{"v":2.744743443,"d":"2.74"}]
["51610","Falls Church City","VA",{"v":1.0453546372023407E-9,"d":"0.00"},{"v":1.0453546372023404E-9,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["51620","Franklin City","VA",{"v":1.6774477511939228,"d":"1.68"},{"v":1.6774477511939225,"d":"1.68"},{"v":0.558918986,"d":"0.56"}]
["51630","Fredericksburg City","VA",{"v":0.017054340441250423,"d":"0.02"},{"v":0.017054340441250423,"d":"0.02"},{"v":1.222083268,"d":"1.22"}]
["51640","Galax City","VA",{"v":2.241923878467121,"d":"2.24"},{"v":2.2419238784671207,"d":"2.24"},{"v":0.828849149,"d":"0.83"}]
["51650","Hampton City","VA",{"v":0.010259252025221743,"d":"0.01"},{"v":0.010259252025221741,"d":"0.01"},{"v":0.58363838,"d":"0.58"}]
["51660","Harrisonburg City","VA",{"v":0.02362632918451314,"d":"0.02"},{"v":0.023626329184513142,"d":"0.02"},{"v":1.719066813,"d":"1.72"}]
["51670","Hopewell City","VA",{"v":0.04953423639360049,"d":"0.05"},{"v":0.049534236393600474,"d":"0.05"},{"v":0.841990191,"d":"0.84"}]
["51678","Lexington City","VA",{"v":0.14962741289315176,"d":"0.15"},{"v":0.14962741289315176,"d":"0.15"},{"v":1.784003543,"d":"1.78"}]
["51680","Lynchburg City","VA",{"v":0.8333744644889397,"d":"0.83"},{"v":0.8333744644889396,"d":"0.83"},{"v":0.9779209469999999,"d":"0.98"}]
["51683","Manassas City","VA",{"v":1.161246680581656E-3,"d":"0.00"},{"v":1.1612466805816558E-3,"d":"0.00"},{"v":3.5856291000000002,"d":"3.59"}]
["51685","Manassas Park City","VA",{"v":2.2515640496938209E-6,"d":"0.00"},{"v":2.2515640496938209E-6,"d":"0.00"},{"v":0.6065071786195857,"d":"0.61"}]
["51690","Martinsville City","VA",{"v":1.1275634532777246,"d":"1.13"},{"v":1.1275634532777246,"d":"1.13"},{"v":0.751454592,"d":"0.75"}]
["51700","Newport News City","VA",{"v":0.01726424315452711,"d":"0.02"},{"v":0.017264243154527112,"d":"0.02"},{"v":0.757454631,"d":"0.76"}]
["51710","Norfolk City","VA",{"v":3.3554187534595469E-5,"d":"0.00"},{"v":3.3554187534595469E-5,"d":"0.00"},{"v":1.8816353309999998,"d":"1.88"}]
["51720","Norton City","VA",{"v":2.617351439684146,"d":"2.62"},{"v":2.6173514396841466,"d":"2.62"},{"v":0.864333763,"d":"0.86"}]
["51730","Petersburg City","VA",{"v":0.786847208215389,"d":"0.79"},{"v":0.7868472082153891,"d":"0.79"},{"v":0.629790946,"d":"0.63"}]
["51735","Poquoson City","VA",{"v":2.177748511794925,"d":"2.18"},{"v":2.177748511794925,"d":"2.18"},{"v":0.222125882,"d":"0.22"}]
["51740","Portsmouth City","VA",{"v":0.006572953966411019,"d":"0.01"},{"v":0.006572953966411019,"d":"0.01"},{"v":0.827891109,"d":"0.83"}]
["51750","Radford","VA",{"v":0.9479403938702625,"d":"0.95"},{"v":0.9479403938702625,"d":"0.95"},{"v":0.8986371860000001,"d":"0.90"}]
["51760","Richmond City","VA",{"v":1.1845131309795197E-4,"d":"0.00"},{"v":1.1845131309795197E-4,"d":"0.00"},{"v":2.000600715,"d":"2.00"}]
["51770","Roanoke City","VA",{"v":0.017820557510270715,"d":"0.02"},{"v":0.01782055751027072,"d":"0.02"},{"v":1.213046862,"d":"1.21"}]
["51775","Salem City","VA",{"v":0.33307687076175846,"d":"0.33"},{"v":0.33307687076175846,"d":"0.33"},{"v":0.963778324,"d":"0.96"}]
["51790","Staunton City","VA",{"v":1.114042930210521,"d":"1.11"},{"v":1.1140429302105213,"d":"1.11"},{"v":0.527306193,"d":"0.53"}]
["51800","Suffolk City","VA",{"v":2.2930875982096506,"d":"2.29"},{"v":2.29308759820965,"d":"2.29"},{"v":0.35833589,"d":"0.36"}]
["51810","Virginia Beach City","VA",{"v":0.3360301270443798,"d":"0.34"},{"v":0.3360301270443798,"d":"0.34"},{"v":0.467223588,"d":"0.47"}]
["51820","Waynesboro City","VA",{"v":0.6640413580823051,"d":"0.66"},{"v":0.664041358082305,"d":"0.66"},{"v":0.770218158,"d":"0.77"}]
["51830","Williamsburg City","VA",{"v":1.1770760285239112,"d":"1.18"},{"v":1.1770760285239112,"d":"1.18"},{"v":0.658981586,"d":"0.66"}]
["51840","Winchester City","VA",{"v":0.004202302467503064,"d":"0.00"},{"v":0.004202302467503064,"d":"0.00"},{"v":1.401470179,"d":"1.40"}]
["53001","Adams","WA",{"v":2.6778004581437442,"d":"2.68"},{"v":2.6778004581437442,"d":"2.68"},{"v":0.398148953,"d":"0.40"}]
["53003","Asotin","WA",{"v":2.636510718943036,"d":"2.64"},{"v":2.6365107189430357,"d":"2.64"},{"v":0.335828849,"d":"0.34"}]
["53005","Benton","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.35571296999999996,"d":"0.36"}]
["53007","Chelan","WA",{"v":3.0713841897654293,"d":"3.07"},{"v":3.0713841897654293,"d":"3.07"},{"v":1.269715714,"d":"1.27"}]
["53009","Clallam","WA",{"v":2.8983876350026283,"d":"2.90"},{"v":2.8983876350026283,"d":"2.90"},{"v":0.895512788,"d":"0.90"}]
["53011","Clark","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.866593156,"d":"0.87"}]
["53013","Columbia","WA",{"v":2.843060477721822,"d":"2.84"},{"v":2.8430604777218225,"d":"2.84"},{"v":0.635158267,"d":"0.64"}]
["53015","Cowlitz","WA",{"v":2.898339851560084,"d":"2.90"},{"v":2.898339851560084,"d":"2.90"},{"v":1.049726199,"d":"1.05"}]
["53017","Douglas","WA",{"v":2.854609594362559,"d":"2.85"},{"v":2.854609594362559,"d":"2.85"},{"v":0.584699151,"d":"0.58"}]
["53019","Ferry","WA",{"v":3.1587525746824205,"d":"3.16"},{"v":3.1587525746824205,"d":"3.16"},{"v":1.755847378,"d":"1.76"}]
["53021","Franklin","WA",{"v":2.6620417953990554,"d":"2.66"},{"v":2.6620417953990554,"d":"2.66"},{"v":0.336008073,"d":"0.34"}]
["53023","Garfield","WA",{"v":2.8592400900887176,"d":"2.86"},{"v":2.859240090088717,"d":"2.86"},{"v":0.7292331650000001,"d":"0.73"}]
["53025","Grant","WA",{"v":2.761334997959268,"d":"2.76"},{"v":2.7613349979592687,"d":"2.76"},{"v":0.471763086,"d":"0.47"}]
["53027","Grays Harbor","WA",{"v":2.8614096721088362,"d":"2.86"},{"v":2.8614096721088362,"d":"2.86"},{"v":0.941995232,"d":"0.94"}]
["53029","Island","WA",{"v":2.5805631922348002,"d":"2.58"},{"v":2.5805631922348,"d":"2.58"},{"v":0.527196493,"d":"0.53"}]
["53031","Jefferson","WA",{"v":2.906067220386005,"d":"2.91"},{"v":2.906067220386005,"d":"2.91"},{"v":1.105443266,"d":"1.11"}]
["53033","King","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.912225742,"d":"0.91"}]
["53035","Kitsap","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.652293013,"d":"0.65"}]
["53037","Kittitas","WA",{"v":2.994569339842498,"d":"2.99"},{"v":2.994569339842498,"d":"2.99"},{"v":1.053798272,"d":"1.05"}]
["53039","Klickitat","WA",{"v":2.689516071525056,"d":"2.69"},{"v":2.689516071525056,"d":"2.69"},{"v":0.563584896,"d":"0.56"}]
["53041","Lewis","WA",{"v":2.947500223193747,"d":"2.95"},{"v":2.9475002231937473,"d":"2.95"},{"v":1.182366952,"d":"1.18"}]
["53043","Lincoln","WA",{"v":2.8684006706501077,"d":"2.87"},{"v":2.8684006706501077,"d":"2.87"},{"v":0.661460118,"d":"0.66"}]
["53045","Mason","WA",{"v":2.9237847318557715,"d":"2.92"},{"v":2.923784731855772,"d":"2.92"},{"v":1.121639234,"d":"1.12"}]
["53047","Okanogan","WA",{"v":2.9536037814642113,"d":"2.95"},{"v":2.9536037814642113,"d":"2.95"},{"v":1.05599186,"d":"1.06"}]
["53049","Pacific","WA",{"v":2.9073349032415177,"d":"2.91"},{"v":2.9073349032415177,"d":"2.91"},{"v":0.934010884,"d":"0.93"}]
["53051","Pend Oreille","WA",{"v":3.208361811667302,"d":"3.21"},{"v":3.208361811667302,"d":"3.21"},{"v":2.037938232,"d":"2.04"}]
["53053","Pierce","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.767696828,"d":"0.77"}]
["53055","San Juan","WA",{"v":2.6795068849634442,"d":"2.68"},{"v":2.6795068849634447,"d":"2.68"},{"v":0.559422423,"d":"0.56"}]
["53057","Skagit","WA",{"v":2.7195406338583608,"d":"2.72"},{"v":2.7195406338583603,"d":"2.72"},{"v":0.654564707,"d":"0.65"}]
["53059","Skamania","WA",{"v":3.2300773674641308,"d":"3.23"},{"v":3.2300773674641308,"d":"3.23"},{"v":2.298873802,"d":"2.30"}]
["53061","Snohomish","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.737376684,"d":"0.74"}]
["53063","Spokane","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.671496157,"d":"0.67"}]
["53065","Stevens","WA",{"v":3.1268195215323256,"d":"3.13"},{"v":3.1268195215323256,"d":"3.13"},{"v":1.45013663,"d":"1.45"}]
["53067","Thurston","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.635018995,"d":"0.64"}]
["53069","Wahkiakum","WA",{"v":2.9392616685351243,"d":"2.94"},{"v":2.9392616685351247,"d":"2.94"},{"v":1.183427671,"d":"1.18"}]
["53071","Walla Walla","WA",{"v":2.5926267878045577,"d":"2.59"},{"v":2.5926267878045577,"d":"2.59"},{"v":0.316192872,"d":"0.32"}]
["53073","Whatcom","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":1.002233296,"d":"1.00"}]
["53075","Whitman","WA",{"v":2.649158836090563,"d":"2.65"},{"v":2.649158836090562,"d":"2.65"},{"v":0.417604953,"d":"0.42"}]
["53077","Yakima","WA",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"v":0.487881894,"d":"0.49"}]
["54001","Barbour","WV",{"v":6.970647821712595,"d":"6.97"},{"v":6.970647821712595,"d":"6.97"},{"v":1.9888064670000003,"d":"1.99"}]
["54003","Berkeley","WV",{"v":7.516781206647624,"d":"7.52"},{"v":7.516781206647624,"d":"7.52"},{"v":1.917899743,"d":"1.92"}]
["54005","Boone","WV",{"v":7.384566730739678,"d":"7.38"},{"v":7.384566730739676,"d":"7.38"},{"v":2.000387832,"d":"2.00"}]
["54007","Braxton","WV",{"v":7.488715042023755,"d":"7.49"},{"v":7.488715042023756,"d":"7.49"},{"v":2.42798634,"d":"2.43"}]
["54009","Brooke","WV",{"v":6.7372487848555656,"d":"6.74"},{"v":6.737248784855565,"d":"6.74"},{"v":1.372473809,"d":"1.37"}]
["54011","Cabell","WV",{"v":6.772622659842244,"d":"6.77"},{"v":6.772622659842244,"d":"6.77"},{"v":1.408766014,"d":"1.41"}]
["54013","Calhoun","WV",{"v":7.241689254989842,"d":"7.24"},{"v":7.241689254989843,"d":"7.24"},{"v":1.985593098,"d":"1.99"}]
["54015","Clay","WV",{"v":7.514399052969055,"d":"7.51"},{"v":7.514399052969054,"d":"7.51"},{"v":2.178305769,"d":"2.18"}]
["54017","Doddridge","WV",{"v":7.105798105905454,"d":"7.11"},{"v":7.105798105905455,"d":"7.11"},{"v":1.839071971,"d":"1.84"}]
["54019","Fayette","WV",{"v":7.639298569170366,"d":"7.64"},{"v":7.639298569170365,"d":"7.64"},{"v":2.641757588,"d":"2.64"}]
["54021","Gilmer","WV",{"v":7.229676822431164,"d":"7.23"},{"v":7.229676822431162,"d":"7.23"},{"v":1.845623625,"d":"1.85"}]
["54023","Grant","WV",{"v":8.138840231779081,"d":"8.14"},{"v":8.138840231779083,"d":"8.14"},{"v":2.604880545,"d":"2.60"}]
["54025","Greenbrier","WV",{"v":7.817499461064465,"d":"7.82"},{"v":7.817499461064465,"d":"7.82"},{"v":2.806307794,"d":"2.81"}]
["54027","Hampshire","WV",{"v":7.46399006926678,"d":"7.46"},{"v":7.46399006926678,"d":"7.46"},{"v":3.001970068,"d":"3.00"}]
["54029","Hancock","WV",{"v":6.662202060877079,"d":"6.66"},{"v":6.662202060877079,"d":"6.66"},{"v":1.426834873,"d":"1.43"}]
["54031","Hardy","WV",{"v":7.872403739594657,"d":"7.87"},{"v":7.872403739594657,"d":"7.87"},{"v":2.928405935,"d":"2.93"}]
["54033","Harrison","WV",{"v":6.656446100733155,"d":"6.66"},{"v":6.656446100733155,"d":"6.66"},{"v":1.320454146,"d":"1.32"}]
["54035","Jackson","WV",{"v":6.678506918252364,"d":"6.68"},{"v":6.6785069182523635,"d":"6.68"},{"v":1.721213025,"d":"1.72"}]
["54037","Jefferson","WV",{"v":7.732489148783172,"d":"7.73"},{"v":7.732489148783174,"d":"7.73"},{"v":1.6983569219999999,"d":"1.70"}]
["54039","Kanawha","WV",{"v":6.607052602180112,"d":"6.61"},{"v":6.607052602180112,"d":"6.61"},{"v":1.570322432,"d":"1.57"}]
["54041","Lewis","WV",{"v":6.980804536452041,"d":"6.98"},{"v":6.98080453645204,"d":"6.98"},{"v":1.754165944,"d":"1.75"}]
["54043","Lincoln","WV",{"v":7.275699598023313,"d":"7.28"},{"v":7.275699598023313,"d":"7.28"},{"v":2.000715311,"d":"2.00"}]
["54045","Logan","WV",{"v":7.449752158817982,"d":"7.45"},{"v":7.449752158817981,"d":"7.45"},{"v":2.030047203,"d":"2.03"}]
["54047","McDowell","WV",{"v":7.926723302750009,"d":"7.93"},{"v":7.926723302750008,"d":"7.93"},{"v":3.015199366,"d":"3.02"}]
["54049","Marion","WV",{"v":6.428735239610279,"d":"6.43"},{"v":6.42873523961028,"d":"6.43"},{"v":1.468700474,"d":"1.47"}]
["54051","Marshall","WV",{"v":7.076053782781544,"d":"7.08"},{"v":7.076053782781545,"d":"7.08"},{"v":1.642736589,"d":"1.64"}]
["54053","Mason","WV",{"v":7.26106959404352,"d":"7.26"},{"v":7.26106959404352,"d":"7.26"},{"v":1.7361676699999997,"d":"1.74"}]
["54055","Mercer","WV",{"v":7.572482805966864,"d":"7.57"},{"v":7.572482805966862,"d":"7.57"},{"v":2.175108429,"d":"2.18"}]
["54057","Mineral","WV",{"v":7.388276105202116,"d":"7.39"},{"v":7.388276105202115,"d":"7.39"},{"v":2.396029813,"d":"2.40"}]
["54059","Mingo","WV",{"v":7.460975837670962,"d":"7.46"},{"v":7.460975837670962,"d":"7.46"},{"v":2.377382793,"d":"2.38"}]
["54061","Monongalia","WV",{"v":6.97017538863132,"d":"6.97"},{"v":6.97017538863132,"d":"6.97"},{"v":1.577373483,"d":"1.58"}]
["54063","Monroe","WV",{"v":7.6713261731791,"d":"7.67"},{"v":7.6713261731791,"d":"7.67"},{"v":2.446094511,"d":"2.45"}]
["54065","Morgan","WV",{"v":7.878322778363551,"d":"7.88"},{"v":7.878322778363551,"d":"7.88"},{"v":3.145087474,"d":"3.15"}]
["54067","Nicholas","WV",{"v":7.801537859920402,"d":"7.80"},{"v":7.801537859920402,"d":"7.80"},{"v":3.0433932940000004,"d":"3.04"}]
["54069","Ohio","WV",{"v":6.488024791757509,"d":"6.49"},{"v":6.488024791757509,"d":"6.49"},{"v":1.309002386,"d":"1.31"}]
["54071","Pendleton","WV",{"v":7.645100256921664,"d":"7.65"},{"v":7.645100256921665,"d":"7.65"},{"v":3.167073703,"d":"3.17"}]
["54073","Pleasants","WV",{"v":6.981314347788963,"d":"6.98"},{"v":6.981314347788963,"d":"6.98"},{"v":1.799431526,"d":"1.80"}]
["54075","Pocahontas","WV",{"v":8.088547877996568,"d":"8.09"},{"v":8.088547877996568,"d":"8.09"},{"v":3.9374898540000003,"d":"3.94"}]
["54077","Preston","WV",{"v":7.856343616649199,"d":"7.86"},{"v":7.8563436166492,"d":"7.86"},{"v":2.989732865,"d":"2.99"}]
["54079","Putnam","WV",{"v":6.520731986786389,"d":"6.52"},{"v":6.520731986786389,"d":"6.52"},{"v":1.613082419,"d":"1.61"}]
["54081","Raleigh","WV",{"v":7.52535047875897,"d":"7.53"},{"v":7.525350478758971,"d":"7.53"},{"v":2.352882369,"d":"2.35"}]
["54083","Randolph","WV",{"v":7.665472204358437,"d":"7.67"},{"v":7.665472204358437,"d":"7.67"},{"v":2.7789967160000004,"d":"2.78"}]
["54085","Ritchie","WV",{"v":6.9000104508898366,"d":"6.90"},{"v":6.9000104508898366,"d":"6.90"},{"v":1.797799259,"d":"1.80"}]
["54087","Roane","WV",{"v":6.939032430041585,"d":"6.94"},{"v":6.939032430041585,"d":"6.94"},{"v":1.78904313,"d":"1.79"}]
["54089","Summers","WV",{"v":7.65040117673751,"d":"7.65"},{"v":7.65040117673751,"d":"7.65"},{"v":2.452065633,"d":"2.45"}]
["54091","Taylor","WV",{"v":6.965826494585926,"d":"6.97"},{"v":6.965826494585926,"d":"6.97"},{"v":1.733106281,"d":"1.73"}]
["54093","Tucker","WV",{"v":7.0831982338238335,"d":"7.08"},{"v":7.083198233823835,"d":"7.08"},{"v":2.729205105,"d":"2.73"}]
["54095","Tyler","WV",{"v":6.987007038436145,"d":"6.99"},{"v":6.987007038436146,"d":"6.99"},{"v":1.867553699,"d":"1.87"}]
["54097","Upshur","WV",{"v":7.213189345018633,"d":"7.21"},{"v":7.213189345018632,"d":"7.21"},{"v":2.010104753,"d":"2.01"}]
["54099","Wayne","WV",{"v":7.375802908007671,"d":"7.38"},{"v":7.375802908007671,"d":"7.38"},{"v":1.863075331,"d":"1.86"}]
["54101","Webster","WV",{"v":8.081624347832266,"d":"8.08"},{"v":8.081624347832266,"d":"8.08"},{"v":4.188436847,"d":"4.19"}]
["54103","Wetzel","WV",{"v":6.87012525747414,"d":"6.87"},{"v":6.8701252574741405,"d":"6.87"},{"v":1.68746689,"d":"1.69"}]
["54105","Wirt","WV",{"v":6.836014330016766,"d":"6.84"},{"v":6.836014330016767,"d":"6.84"},{"v":2.192504163,"d":"2.19"}]
["54107","Wood","WV",{"v":6.06016695837467,"d":"6.06"},{"v":6.060166958374669,"d":"6.06"},{"v":1.360889389,"d":"1.36"}]
["54109","Wyoming","WV",{"v":7.65879672115946,"d":"7.66"},{"v":7.658796721159461,"d":"7.66"},{"v":2.62259207,"d":"2.62"}]
["55001","Adams","WI",{"v":4.821845348122881,"d":"4.82"},{"v":4.821845348122881,"d":"4.82"},{"v":1.651908585,"d":"1.65"}]
["55003","Ashland","WI",{"v":4.498716873193827,"d":"4.50"},{"v":4.498716873193827,"d":"4.50"},{"v":1.932922656,"d":"1.93"}]
["55005","Barron","WI",{"v":4.401314482011449,"d":"4.40"},{"v":4.401314482011449,"d":"4.40"},{"v":1.716961524,"d":"1.72"}]
["55007","Bayfield","WI",{"v":4.431903411043024,"d":"4.43"},{"v":4.431903411043023,"d":"4.43"},{"v":2.841834042,"d":"2.84"}]
["55009","Brown","WI",{"v":3.77411069421961,"d":"3.77"},{"v":3.774110694219611,"d":"3.77"},{"v":0.754675596,"d":"0.75"}]
["55011","Buffalo","WI",{"v":4.405744153435224,"d":"4.41"},{"v":4.405744153435225,"d":"4.41"},{"v":1.9381020490000003,"d":"1.94"}]
["55013","Burnett","WI",{"v":4.509735381340038,"d":"4.51"},{"v":4.509735381340038,"d":"4.51"},{"v":2.43079352,"d":"2.43"}]
["55015","Calumet","WI",{"v":3.9234343050961664,"d":"3.92"},{"v":3.9234343050961664,"d":"3.92"},{"v":0.692085066,"d":"0.69"}]
["55017","Chippewa","WI",{"v":4.847213673019015,"d":"4.85"},{"v":4.847213673019014,"d":"4.85"},{"v":1.617810219,"d":"1.62"}]
["55019","Clark","WI",{"v":4.491755809714013,"d":"4.49"},{"v":4.491755809714013,"d":"4.49"},{"v":2.118729625,"d":"2.12"}]
["55021","Columbia","WI",{"v":4.166917139676129,"d":"4.17"},{"v":4.166917139676129,"d":"4.17"},{"v":0.856113333,"d":"0.86"}]
["55023","Crawford","WI",{"v":4.388421576829048,"d":"4.39"},{"v":4.388421576829048,"d":"4.39"},{"v":1.231120329,"d":"1.23"}]
["55025","Dane","WI",{"v":3.7247780078275032,"d":"3.72"},{"v":3.724778007827503,"d":"3.72"},{"v":0.695374721,"d":"0.70"}]
["55027","Dodge","WI",{"v":3.733540160837245,"d":"3.73"},{"v":3.733540160837245,"d":"3.73"},{"v":0.698019556,"d":"0.70"}]
["55029","Door","WI",{"v":3.5999790679286643,"d":"3.60"},{"v":3.5999790679286643,"d":"3.60"},{"v":0.979619831,"d":"0.98"}]
["55031","Douglas","WI",{"v":4.5614564782040645,"d":"4.56"},{"v":4.5614564782040645,"d":"4.56"},{"v":1.712790746,"d":"1.71"}]
["55033","Dunn","WI",{"v":4.5438503866090505,"d":"4.54"},{"v":4.543850386609051,"d":"4.54"},{"v":1.369276751,"d":"1.37"}]
["55035","Eau Claire","WI",{"v":4.623834780491591,"d":"4.62"},{"v":4.623834780491591,"d":"4.62"},{"v":1.435188419,"d":"1.44"}]
["55037","Florence","WI",{"v":4.76963869780599,"d":"4.77"},{"v":4.769638697805991,"d":"4.77"},{"v":2.829313034,"d":"2.83"}]
["55039","Fond Du Lac","WI",{"v":3.678077224172456,"d":"3.68"},{"v":3.678077224172456,"d":"3.68"},{"v":0.740299499,"d":"0.74"}]
["55041","Forest","WI",{"v":4.819291169733971,"d":"4.82"},{"v":4.8192911697339715,"d":"4.82"},{"v":2.895312483,"d":"2.90"}]
["55043","Grant","WI",{"v":4.174027844014762,"d":"4.17"},{"v":4.174027844014763,"d":"4.17"},{"v":0.9732084560000002,"d":"0.97"}]
["55045","Green","WI",{"v":4.085957279806142,"d":"4.09"},{"v":4.085957279806143,"d":"4.09"},{"v":0.793951755,"d":"0.79"}]
["55047","Green Lake","WI",{"v":3.4374957831595245,"d":"3.44"},{"v":3.4374957831595245,"d":"3.44"},{"v":0.9523488550000001,"d":"0.95"}]
["55049","Iowa","WI",{"v":4.0683509610473845,"d":"4.07"},{"v":4.0683509610473845,"d":"4.07"},{"v":1.102598235,"d":"1.10"}]
["55051","Iron","WI",{"v":4.711461999744378,"d":"4.71"},{"v":4.711461999744377,"d":"4.71"},{"v":2.620401593,"d":"2.62"}]
["55053","Jackson","WI",{"v":3.956847335235827,"d":"3.96"},{"v":3.956847335235827,"d":"3.96"},{"v":1.726502545,"d":"1.73"}]
["55055","Jefferson","WI",{"v":4.098614779802164,"d":"4.10"},{"v":4.098614779802165,"d":"4.10"},{"v":0.692036363,"d":"0.69"}]
["55057","Juneau","WI",{"v":4.617947817074804,"d":"4.62"},{"v":4.6179478170748025,"d":"4.62"},{"v":1.507012306,"d":"1.51"}]
["55059","Kenosha","WI",{"v":3.71416500369749,"d":"3.71"},{"v":3.71416500369749,"d":"3.71"},{"v":0.650616427,"d":"0.65"}]
["55061","Kewaunee","WI",{"v":3.967004605103065,"d":"3.97"},{"v":3.9670046051030656,"d":"3.97"},{"v":0.933747431,"d":"0.93"}]
["55063","La Crosse","WI",{"v":3.6181750511291155,"d":"3.62"},{"v":3.618175051129116,"d":"3.62"},{"v":1.153041668,"d":"1.15"}]
["55065","Lafayette","WI",{"v":4.05817316848706,"d":"4.06"},{"v":4.05817316848706,"d":"4.06"},{"v":0.95398637,"d":"0.95"}]
["55067","Langlade","WI",{"v":4.526416548370501,"d":"4.53"},{"v":4.5264165483705,"d":"4.53"},{"v":2.076523662,"d":"2.08"}]
["55069","Lincoln","WI",{"v":4.385247831615334,"d":"4.39"},{"v":4.385247831615333,"d":"4.39"},{"v":2.289883824,"d":"2.29"}]
["55071","Manitowoc","WI",{"v":3.729516705446058,"d":"3.73"},{"v":3.729516705446057,"d":"3.73"},{"v":0.750341492,"d":"0.75"}]
["55073","Marathon","WI",{"v":4.494642386944588,"d":"4.49"},{"v":4.494642386944588,"d":"4.49"},{"v":1.610983133,"d":"1.61"}]
["55075","Marinette","WI",{"v":4.733706159597491,"d":"4.73"},{"v":4.7337061595974905,"d":"4.73"},{"v":2.080037967,"d":"2.08"}]
["55077","Marquette","WI",{"v":4.758645787169702,"d":"4.76"},{"v":4.758645787169703,"d":"4.76"},{"v":1.411858233,"d":"1.41"}]
["55078","Menominee","WI",{"v":5.462992367577615,"d":"5.46"},{"v":5.462992367577616,"d":"5.46"},{"v":3.769400598,"d":"3.77"}]
["55079","Milwaukee","WI",{"v":6.58485074185036e-05,"d":"0.00"},{"v":6.5848507418503615E-5,"d":"0.00"},{"v":4.176434951,"d":"4.18"}]
["55081","Monroe","WI",{"v":4.707785003914139,"d":"4.71"},{"v":4.707785003914139,"d":"4.71"},{"v":1.363576956,"d":"1.36"}]
["55083","Oconto","WI",{"v":4.660925678701248,"d":"4.66"},{"v":4.660925678701248,"d":"4.66"},{"v":1.963254669,"d":"1.96"}]
["55085","Oneida","WI",{"v":4.627153456232442,"d":"4.63"},{"v":4.627153456232442,"d":"4.63"},{"v":2.153139289,"d":"2.15"}]
["55087","Outagamie","WI",{"v":4.028094632065141,"d":"4.03"},{"v":4.028094632065141,"d":"4.03"},{"v":0.771632111,"d":"0.77"}]
["55089","Ozaukee","WI",{"v":3.8191461234989514,"d":"3.82"},{"v":3.8191461234989514,"d":"3.82"},{"v":0.656217432,"d":"0.66"}]
["55091","Pepin","WI",{"v":4.335550069800062,"d":"4.34"},{"v":4.335550069800063,"d":"4.34"},{"v":1.631708347,"d":"1.63"}]
["55093","Pierce","WI",{"v":4.234885897338053,"d":"4.23"},{"v":4.234885897338054,"d":"4.23"},{"v":1.16431712,"d":"1.16"}]
["55095","Polk","WI",{"v":4.610132121050824,"d":"4.61"},{"v":4.610132121050825,"d":"4.61"},{"v":2.026977065,"d":"2.03"}]
["55097","Portage","WI",{"v":4.191611240234705,"d":"4.19"},{"v":4.191611240234705,"d":"4.19"},{"v":1.051303626,"d":"1.05"}]
["55099","Price","WI",{"v":4.8177553830628375,"d":"4.82"},{"v":4.8177553830628375,"d":"4.82"},{"v":2.913867243,"d":"2.91"}]
["55101","Racine","WI",{"v":3.573733263318943,"d":"3.57"},{"v":3.573733263318943,"d":"3.57"},{"v":0.645733988,"d":"0.65"}]
["55103","Richland","WI",{"v":4.280603555277349,"d":"4.28"},{"v":4.280603555277349,"d":"4.28"},{"v":1.302307728,"d":"1.30"}]
["55105","Rock","WI",{"v":3.9735042923459285,"d":"3.97"},{"v":3.9735042923459294,"d":"3.97"},{"v":0.604958828,"d":"0.60"}]
["55107","Rusk","WI",{"v":4.81980938263007,"d":"4.82"},{"v":4.81980938263007,"d":"4.82"},{"v":2.518763032,"d":"2.52"}]
["55109","St Croix","WI",{"v":4.4257854954530345,"d":"4.43"},{"v":4.4257854954530345,"d":"4.43"},{"v":0.9863485380000001,"d":"0.99"}]
["55111","Sauk","WI",{"v":4.005073098547436,"d":"4.01"},{"v":4.005073098547436,"d":"4.01"},{"v":0.987490521,"d":"0.99"}]
["55113","Sawyer","WI",{"v":4.613528259141189,"d":"4.61"},{"v":4.613528259141189,"d":"4.61"},{"v":3.157882151,"d":"3.16"}]
["55115","Shawano","WI",{"v":4.713682180821303,"d":"4.71"},{"v":4.713682180821303,"d":"4.71"},{"v":1.890426769,"d":"1.89"}]
["55117","Sheboygan","WI",{"v":3.8350290455970026,"d":"3.84"},{"v":3.835029045597003,"d":"3.84"},{"v":0.745382292,"d":"0.75"}]
["55119","Taylor","WI",{"v":4.581826507366484,"d":"4.58"},{"v":4.581826507366484,"d":"4.58"},{"v":2.589599168,"d":"2.59"}]
["55121","Trempealeau","WI",{"v":4.434641971849477,"d":"4.43"},{"v":4.434641971849477,"d":"4.43"},{"v":1.446180548,"d":"1.45"}]
["55123","Vernon","WI",{"v":4.207182859226018,"d":"4.21"},{"v":4.207182859226018,"d":"4.21"},{"v":1.307194973,"d":"1.31"}]
["55125","Vilas","WI",{"v":4.1968984790467445,"d":"4.20"},{"v":4.1968984790467445,"d":"4.20"},{"v":2.655779777,"d":"2.66"}]
["55127","Walworth","WI",{"v":4.1278839615557965,"d":"4.13"},{"v":4.127883961555796,"d":"4.13"},{"v":0.648405324,"d":"0.65"}]
["55129","Washburn","WI",{"v":4.688089979583907,"d":"4.69"},{"v":4.688089979583906,"d":"4.69"},{"v":2.624887841,"d":"2.62"}]
["55131","Washington","WI",{"v":3.965597680035673,"d":"3.97"},{"v":3.9655976800356734,"d":"3.97"},{"v":0.726618084,"d":"0.73"}]
["55133","Waukesha","WI",{"v":3.256360071852236,"d":"3.26"},{"v":3.2563600718522365,"d":"3.26"},{"v":0.765192613,"d":"0.77"}]
["55135","Waupaca","WI",{"v":4.143209429393179,"d":"4.14"},{"v":4.1432094293931785,"d":"4.14"},{"v":1.3648023950000001,"d":"1.36"}]
["55137","Waushara","WI",{"v":4.6346446552021545,"d":"4.63"},{"v":4.634644655202154,"d":"4.63"},{"v":1.430685172,"d":"1.43"}]
["55139","Winnebago","WI",{"v":3.639217230527698,"d":"3.64"},{"v":3.6392172305276986,"d":"3.64"},{"v":0.667236548,"d":"0.67"}]
["55141","Wood","WI",{"v":4.083925127161918,"d":"4.08"},{"v":4.083925127161918,"d":"4.08"},{"v":1.002128237,"d":"1.00"}]
["56001","Albany","WY",{"v":1.7350416432194729,"d":"1.74"},{"v":1.7350416432194726,"d":"1.74"},{"v":0.36813142,"d":"0.37"}]
["56003","Big Horn","WY",{"v":1.8695507286390323,"d":"1.87"},{"v":1.869550728639032,"d":"1.87"},{"v":0.530742213,"d":"0.53"}]
["56005","Campbell","WY",{"v":1.8160501945111545,"d":"1.82"},{"v":1.8160501945111547,"d":"1.82"},{"v":0.403358222,"d":"0.40"}]
["56007","Carbon","WY",{"v":1.810388291321929,"d":"1.81"},{"v":1.8103882913219291,"d":"1.81"},{"v":0.463039532,"d":"0.46"}]
["56009","Converse","WY",{"v":1.7366196787364365,"d":"1.74"},{"v":1.736619678736436,"d":"1.74"},{"v":0.359678255,"d":"0.36"}]
["56011","Crook","WY",{"v":1.8782505073229676,"d":"1.88"},{"v":1.8782505073229676,"d":"1.88"},{"v":0.778564931,"d":"0.78"}]
["56013","Fremont","WY",{"v":1.8284479095397492,"d":"1.83"},{"v":1.828447909539749,"d":"1.83"},{"v":0.532036967,"d":"0.53"}]
["56015","Goshen","WY",{"v":1.717332120900681,"d":"1.72"},{"v":1.7173321209006813,"d":"1.72"},{"v":0.324755522,"d":"0.32"}]
["56017","Hot Springs","WY",{"v":1.7712034069295755,"d":"1.77"},{"v":1.7712034069295755,"d":"1.77"},{"v":0.412278752,"d":"0.41"}]
["56019","Johnson","WY",{"v":1.8510222488415038,"d":"1.85"},{"v":1.851022248841504,"d":"1.85"},{"v":0.4492187,"d":"0.45"}]
["56021","Laramie","WY",{"v":1.6845335209087249,"d":"1.68"},{"v":1.684533520908725,"d":"1.68"},{"v":0.260740977,"d":"0.26"}]
["56023","Lincoln","WY",{"v":1.8757684290851038,"d":"1.88"},{"v":1.875768429085104,"d":"1.88"},{"v":0.780305799,"d":"0.78"}]
["56025","Natrona","WY",{"v":1.662880652708754,"d":"1.66"},{"v":1.6628806527087543,"d":"1.66"},{"v":0.249236736,"d":"0.25"}]
["56027","Niobrara","WY",{"v":1.7765403653016607,"d":"1.78"},{"v":1.776540365301661,"d":"1.78"},{"v":0.475407952,"d":"0.48"}]
["56029","Park","WY",{"v":1.8046282258111133,"d":"1.80"},{"v":1.8046282258111133,"d":"1.80"},{"v":0.485506882,"d":"0.49"}]
["56031","Platte","WY",{"v":1.7407024960202242,"d":"1.74"},{"v":1.740702496020224,"d":"1.74"},{"v":0.372631062,"d":"0.37"}]
["56033","Sheridan","WY",{"v":1.7660676595467453,"d":"1.77"},{"v":1.7660676595467453,"d":"1.77"},{"v":0.438525878,"d":"0.44"}]
["56035","Sublette","WY",{"v":1.8613169981633249,"d":"1.86"},{"v":1.8613169981633249,"d":"1.86"},{"v":0.747822632,"d":"0.75"}]
["56037","Sweetwater","WY",{"v":1.777640517947399,"d":"1.78"},{"v":1.777640517947399,"d":"1.78"},{"v":0.323294236,"d":"0.32"}]
["56039","Teton","WY",{"v":2.0059139391498113,"d":"2.01"},{"v":2.0059139391498113,"d":"2.01"},{"v":1.359970995,"d":"1.36"}]
["56041","Uinta","WY",{"v":1.8261056861535232,"d":"1.83"},{"v":1.826105686153523,"d":"1.83"},{"v":0.474889987,"d":"0.47"}]
["56043","Washakie","WY",{"v":1.778758437387658,"d":"1.78"},{"v":1.778758437387658,"d":"1.78"},{"v":0.39689176100000007,"d":"0.40"}]
["56045","Weston","WY",{"v":1.7716263588121026,"d":"1.77"},{"v":1.7716263588121028,"d":"1.77"},{"v":0.461881205,"d":"0.46"}]
["Grand Total",null,null,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]

{"sheet":"NEI-activity_data","index":10,"n_rows":47131,"n_cols":21,"rows_kept":4500,"cut":true,"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["StateAndCountyFIPSCode","StateFIPS","PostalStateCode","CountyFIPS","CountyName","CountyType","SourceClassificationCode","SourceClassificationCodeDescription","Appliance Type","TotalAppliances","ReportingPeriodTypeCode","CalculationDataSource","CalculationDataYear","CalculationMaterialCode","CalculationParameterTypeCode","CalculationParameterValue","CalculationParameterUnitofMeasure","EmissionCalculationMethodCode","Burn rate - TONS WOOD PER APPLIANCE PER COUNTY","cords per ton","Burn Rate - CORDS WOOD PER APPLIANCE PER COUNTY"]
["01001","01","AL","001","Autauga","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",81.77913789083003,"A","CEC Survey",2017,15,"I",127.05816093655504,"TON",8,{"$f":"P2/J2","v":{"v":1.5536744971091483,"d":"1.55"}},{"$f":"VLOOKUP(A2,cordwood_density!A:D,4,FALSE)","v":1.3062},{"$f":"S2/T2","v":{"v":1.1894614125778198,"d":"1.19"}}]
["01001","01","AL","001","Autauga","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.6307409100673,"A","CEC Survey",2017,15,"I",10.302013048909869,"TON",8,{"$f":"P3/J3","v":{"v":1.5536744971091483,"d":"1.55"}},{"$f":"VLOOKUP(A3,cordwood_density!A:D,4,FALSE)","v":1.3062},{"$f":"S3/T3","v":{"v":1.1894614125778198,"d":"1.19"}}]
["01001","01","AL","001","Autauga","","2104008610","Hydronic heater: outdoor","Hydronic heater",79.56889092080759,"A","CEC Survey",2017,15,"I",123.62415658691842,"TON",8,{"v":1.5536744971091485,"d":"1.55"},{"$f":"VLOOKUP(A4,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":1.18946141257782,"d":"1.19"}]
["01001","01","AL","001","Autauga","","2104008620","Hydronic heater: indoor","Hydronic heater",50.83568031051597,"A","CEC Survey",2017,15,"I",78.98210004164233,"TON",8,{"v":1.5536744971091483,"d":"1.55"},{"$f":"VLOOKUP(A5,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":1.1894614125778198,"d":"1.19"}]
["01001","01","AL","001","Autauga","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.210246970022433,"A","CEC Survey",2017,15,"I",3.434004349636623,"TON",8,{"v":1.5536744971091485,"d":"1.55"},{"$f":"VLOOKUP(A6,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":1.18946141257782,"d":"1.19"}]
["01001","01","AL","001","Autauga","","2104008100","Fireplace: general","Fireplace: general",2711.8333313939997,"A","CEC Survey",2017,15,"I",667.7041164366634,"TON",8,{"v":0.24621871436819998,"d":"0.25"},{"$f":"VLOOKUP(A7,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.18850001099999997,"d":"0.19"}]
["01001","01","AL","001","Autauga","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",508.96441401036,"A","CEC Survey",2017,15,"I",269.5523786124008,"TON",8,{"v":0.5296094799408,"d":"0.53"},{"$f":"VLOOKUP(A8,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.405458184,"d":"0.41"}]
["01001","01","AL","001","Autauga","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",673.1464830459599,"A","CEC Survey",2017,15,"I",356.5047588099494,"TON",8,{"v":0.5296094799408,"d":"0.53"},{"$f":"VLOOKUP(A9,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.405458184,"d":"0.41"}]
["01001","01","AL","001","Autauga","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",459.70979329968003,"A","CEC Survey",2017,15,"I",243.4666645531362,"TON",8,{"v":0.5296094799408,"d":"0.53"},{"$f":"VLOOKUP(A10,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.405458184,"d":"0.41"}]
["01001","01","AL","001","Autauga","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3105.4043013180003,"A","CEC Survey",2017,15,"I",600.9339395791566,"TON",8,{"v":0.19351230347820003,"d":"0.19"},{"$f":"VLOOKUP(A11,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.14814906100000003,"d":"0.15"}]
["01001","01","AL","001","Autauga","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",672.760526592,"A","CEC Survey",2017,15,"I",133.03991120855545,"TON",8,{"v":0.197752255,"d":"0.20"},{"$f":"VLOOKUP(A12,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.15139508115143163,"d":"0.15"}]
["01001","01","AL","001","Autauga","","2104009000","Wax Log; Total: All Combustor Types",null,302.39801620726377,"A","CEC Survey",2017,15,"I",103.85217270854034,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A13,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.2629220257234727,"d":"0.26"}]
["01001","01","AL","001","Autauga","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",620.4783225748799,"A","CEC Survey",2017,15,"I",542.109057305203,"TON",8,{"v":0.8736954017274,"d":"0.87"},{"$f":"VLOOKUP(A14,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.668883327,"d":"0.67"}]
["01001","01","AL","001","Autauga","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",820.6326201796799,"A","CEC Survey",2017,15,"I",716.9829467584943,"TON",8,{"v":0.8736954017274001,"d":"0.87"},{"$f":"VLOOKUP(A15,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.6688833270000001,"d":"0.67"}]
["01001","01","AL","001","Autauga","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",560.43203329344,"A","CEC Survey",2017,15,"I",489.6468904692157,"TON",8,{"v":0.8736954017274,"d":"0.87"},{"$f":"VLOOKUP(A16,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.668883327,"d":"0.67"}]
["01003","01","AL","003","Baldwin","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",181.16374396971054,"A","CEC Survey",2017,15,"I",257.8849596955689,"TON",8,{"v":1.4234910034685841,"d":"1.42"},{"$f":"VLOOKUP(A17,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":1.1469591519366562,"d":"1.15"}]
["01003","01","AL","003","Baldwin","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.688952213760313,"A","CEC Survey",2017,15,"I",20.90959132666775,"TON",8,{"v":1.4234910034685844,"d":"1.42"},{"$f":"VLOOKUP(A18,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":1.1469591519366564,"d":"1.15"}]
["01003","01","AL","003","Baldwin","","2104008610","Hydronic heater: outdoor","Hydronic heater",176.26742656512377,"A","CEC Survey",2017,15,"I",250.91509592001302,"TON",8,{"v":1.4234910034685841,"d":"1.42"},{"$f":"VLOOKUP(A19,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":1.1469591519366562,"d":"1.15"}]
["01003","01","AL","003","Baldwin","","2104008620","Hydronic heater: indoor","Hydronic heater",112.61530030549575,"A","CEC Survey",2017,15,"I",160.30686683778612,"TON",8,{"v":1.4234910034685844,"d":"1.42"},{"$f":"VLOOKUP(A20,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":1.1469591519366564,"d":"1.15"}]
["01003","01","AL","003","Baldwin","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.896317404586772,"A","CEC Survey",2017,15,"I",6.969863775555917,"TON",8,{"v":1.4234910034685841,"d":"1.42"},{"$f":"VLOOKUP(A21,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":1.1469591519366562,"d":"1.15"}]
["01003","01","AL","003","Baldwin","","2104008100","Fireplace: general","Fireplace: general",5541.7270083739995,"A","CEC Survey",2017,15,"I",1311.279355280486,"TON",8,{"v":0.23661926206380005,"d":"0.24"},{"$f":"VLOOKUP(A22,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.19065285800000004,"d":"0.19"}]
["01003","01","AL","003","Baldwin","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1726.2180354546,"A","CEC Survey",2017,15,"I",757.6234189179216,"TON",8,{"v":0.4388920769898,"d":"0.44"},{"$f":"VLOOKUP(A23,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.353631518,"d":"0.35"}]
["01003","01","AL","003","Baldwin","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2283.0625630206,"A","CEC Survey",2017,15,"I",1002.0180701817674,"TON",8,{"v":0.43889207698980004,"d":"0.44"},{"$f":"VLOOKUP(A24,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.353631518,"d":"0.35"}]
["01003","01","AL","003","Baldwin","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1559.1646771848002,"A","CEC Survey",2017,15,"I",684.3050235387681,"TON",8,{"v":0.43889207698980004,"d":"0.44"},{"$f":"VLOOKUP(A25,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.353631518,"d":"0.35"}]
["01003","01","AL","003","Baldwin","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,9443.132749238,"A","CEC Survey",2017,15,"I",1730.732445610123,"TON",8,{"v":0.18327947849190004,"d":"0.18"},{"$f":"VLOOKUP(A26,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.147675029,"d":"0.15"}]
["01003","01","AL","003","Baldwin","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2091.270806583,"A","CEC Survey",2017,15,"I",307.02820862642176,"TON",8,{"v":0.14681418,"d":"0.15"},{"$f":"VLOOKUP(A27,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.11829359439207153,"d":"0.12"}]
["01003","01","AL","003","Baldwin","","2104009000","Wax Log; Total: All Combustor Types",null,1093.4961607251646,"A","CEC Survey",2017,15,"I",256.02277115175247,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A28,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.1886490210297317,"d":"0.19"}]
["01003","01","AL","003","Baldwin","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1943.3785461761101,"A","CEC Survey",2017,15,"I",1478.3604353366952,"TON",8,{"v":0.7607166592662,"d":"0.76"},{"$f":"VLOOKUP(A29,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.612937442,"d":"0.61"}]
["01003","01","AL","003","Baldwin","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2570.27485139421,"A","CEC Survey",2017,15,"I",1955.2508983485322,"TON",8,{"v":0.7607166592662,"d":"0.76"},{"$f":"VLOOKUP(A30,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.612937442,"d":"0.61"}]
["01003","01","AL","003","Baldwin","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1755.3096546106804,"A","CEC Survey",2017,15,"I",1335.2932964331442,"TON",8,{"v":0.7607166592662,"d":"0.76"},{"$f":"VLOOKUP(A31,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.612937442,"d":"0.61"}]
["01005","01","AL","005","Barbour","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",35.66582736332909,"A","CEC Survey",2017,15,"I",55.38768586872281,"TON",8,{"v":1.552962316126482,"d":"1.55"},{"$f":"VLOOKUP(A32,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":1.2017041833370596,"d":"1.20"}]
["01005","01","AL","005","Barbour","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.8918238402699266,"A","CEC Survey",2017,15,"I",4.4908934488153625,"TON",8,{"v":1.5529623161264818,"d":"1.55"},{"$f":"VLOOKUP(A33,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":1.2017041833370594,"d":"1.20"}]
["01005","01","AL","005","Barbour","","2104008610","Hydronic heater: outdoor","Hydronic heater",34.70188608323912,"A","CEC Survey",2017,15,"I",53.89072138578435,"TON",8,{"v":1.552962316126482,"d":"1.55"},{"$f":"VLOOKUP(A34,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":1.2017041833370596,"d":"1.20"}]
["01005","01","AL","005","Barbour","","2104008620","Hydronic heater: indoor","Hydronic heater",22.17064944206944,"A","CEC Survey",2017,15,"I",34.430183107584455,"TON",8,{"v":1.552962316126482,"d":"1.55"},{"$f":"VLOOKUP(A35,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":1.2017041833370596,"d":"1.20"}]
["01005","01","AL","005","Barbour","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9639412800899756,"A","CEC Survey",2017,15,"I",1.4969644829384543,"TON",8,{"v":1.5529623161264818,"d":"1.55"},{"$f":"VLOOKUP(A36,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":1.2017041833370594,"d":"1.20"}]
["01005","01","AL","005","Barbour","","2104008100","Fireplace: general","Fireplace: general",779.1342407029999,"A","CEC Survey",2017,15,"I",204.09711685797703,"TON",8,{"v":0.26195372529620004,"d":"0.26"},{"$f":"VLOOKUP(A37,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.20270349400000004,"d":"0.20"}]
["01005","01","AL","005","Barbour","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",270.95765716383,"A","CEC Survey",2017,15,"I",150.29002217484492,"TON",8,{"v":0.5546623917108,"d":"0.55"},{"$f":"VLOOKUP(A38,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.429205596,"d":"0.43"}]
["01005","01","AL","005","Barbour","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",358.36335302313,"A","CEC Survey",2017,15,"I",198.77067448931103,"TON",8,{"v":0.5546623917108,"d":"0.55"},{"$f":"VLOOKUP(A39,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.429205596,"d":"0.43"}]
["01005","01","AL","005","Barbour","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",244.73594840604002,"A","CEC Survey",2017,15,"I",135.74582648050512,"TON",8,{"v":0.5546623917108,"d":"0.55"},{"$f":"VLOOKUP(A40,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.429205596,"d":"0.43"}]
["01005","01","AL","005","Barbour","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1209.0116946179999,"A","CEC Survey",2017,15,"I",226.9526325991578,"TON",8,{"v":0.18771748330429996,"d":"0.19"},{"$f":"VLOOKUP(A41,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.14525844099999996,"d":"0.15"}]
["01005","01","AL","005","Barbour","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",266.647950114,"A","CEC Survey",2017,15,"I",62.0731728265773,"TON",8,{"v":0.232790737,"d":"0.23"},{"$f":"VLOOKUP(A42,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.1801367615878666,"d":"0.18"}]
["01005","01","AL","005","Barbour","","2104009000","Wax Log; Total: All Combustor Types",null,132.01007727562276,"A","CEC Survey",2017,15,"I",30.90782301571929,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A43,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.1811748819933452,"d":"0.18"}]
["01005","01","AL","005","Barbour","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",317.94061150761,"A","CEC Survey",2017,15,"I",300.73066945784717,"TON",8,{"v":0.9458705763690999,"d":"0.95"},{"$f":"VLOOKUP(A44,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.7319280169999999,"d":"0.73"}]
["01005","01","AL","005","Barbour","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",420.50209909071,"A","CEC Survey",2017,15,"I",397.74056283134627,"TON",8,{"v":0.9458705763691001,"d":"0.95"},{"$f":"VLOOKUP(A45,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.7319280170000001,"d":"0.73"}]
["01005","01","AL","005","Barbour","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",287.1721652326801,"A","CEC Survey",2017,15,"I",271.62770144579747,"TON",8,{"v":0.9458705763690999,"d":"0.95"},{"$f":"VLOOKUP(A46,cordwood_density!A:D,4,FALSE)","v":1.2923},{"v":0.7319280169999999,"d":"0.73"}]
["01007","01","AL","007","Bibb","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",42.776249544044425,"A","CEC Survey",2017,15,"I",72.44048822896978,"TON",8,{"v":1.6934745098300792,"d":"1.69"},{"$f":"VLOOKUP(A47,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":1.253218759587123,"d":"1.25"}]
["01007","01","AL","007","Bibb","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.468344557625224,"A","CEC Survey",2017,15,"I",5.873553099646199,"TON",8,{"v":1.6934745098300792,"d":"1.69"},{"$f":"VLOOKUP(A48,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":1.253218759587123,"d":"1.25"}]
["01007","01","AL","007","Bibb","","2104008610","Hydronic heater: outdoor","Hydronic heater",41.620134691502685,"A","CEC Survey",2017,15,"I",70.48263719575438,"TON",8,{"v":1.6934745098300792,"d":"1.69"},{"$f":"VLOOKUP(A49,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":1.253218759587123,"d":"1.25"}]
["01007","01","AL","007","Bibb","","2104008620","Hydronic heater: indoor","Hydronic heater",26.59064160846005,"A","CEC Survey",2017,15,"I",45.030573763954195,"TON",8,{"v":1.6934745098300792,"d":"1.69"},{"$f":"VLOOKUP(A50,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":1.253218759587123,"d":"1.25"}]
["01007","01","AL","007","Bibb","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.1561148525417413,"A","CEC Survey",2017,15,"I",1.9578510332153998,"TON",8,{"v":1.6934745098300794,"d":"1.69"},{"$f":"VLOOKUP(A51,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":1.2532187595871231,"d":"1.25"}]
["01007","01","AL","007","Bibb","","2104008100","Fireplace: general","Fireplace: general",838.4654650492356,"A","CEC Survey",2017,15,"I",226.54436760393403,"TON",8,{"v":0.2701892648502,"d":"0.27"},{"$f":"VLOOKUP(A52,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.199947654,"d":"0.20"}]
["01007","01","AL","007","Bibb","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",217.82676482349606,"A","CEC Survey",2017,15,"I",144.7435656201893,"TON",8,{"v":0.6644893511477998,"d":"0.66"},{"$f":"VLOOKUP(A53,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.4917408059999999,"d":"0.49"}]
["01007","01","AL","007","Bibb","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",288.0934631536561,"A","CEC Survey",2017,15,"I",191.4350384008955,"TON",8,{"v":0.6644893511477998,"d":"0.66"},{"$f":"VLOOKUP(A54,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.4917408059999999,"d":"0.49"}]
["01007","01","AL","007","Bibb","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",196.7467553244481,"A","CEC Survey",2017,15,"I",130.73612378597744,"TON",8,{"v":0.6644893511477998,"d":"0.66"},{"$f":"VLOOKUP(A55,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.4917408059999999,"d":"0.49"}]
["01007","01","AL","007","Bibb","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1052.4656278201785,"A","CEC Survey",2017,15,"I",209.9464456088303,"TON",8,{"v":0.19948057215289997,"d":"0.20"},{"$f":"VLOOKUP(A56,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.147621233,"d":"0.15"}]
["01007","01","AL","007","Bibb","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",246.66924431166646,"A","CEC Survey",2017,15,"I",76.77505414418819,"TON",8,{"v":0.311246967,"d":"0.31"},{"$f":"VLOOKUP(A57,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.23033150817731074,"d":"0.23"}]
["01007","01","AL","007","Bibb","","2104009000","Wax Log; Total: All Combustor Types",null,57.95794732838028,"A","CEC Survey",2017,15,"I",19.90442540355148,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A58,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.2541469325834382,"d":"0.25"}]
["01007","01","AL","007","Bibb","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",288.0418257387286,"A","CEC Survey",2017,15,"I",301.4864096955917,"TON",8,{"v":1.0466758045376998,"d":"1.05"},{"$f":"VLOOKUP(A59,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.7745695289999999,"d":"0.77"}]
["01007","01","AL","007","Bibb","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",380.9585437189636,"A","CEC Survey",2017,15,"I",398.7400902425568,"TON",8,{"v":1.0466758045377,"d":"1.05"},{"$f":"VLOOKUP(A60,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.7745695290000001,"d":"0.77"}]
["01007","01","AL","007","Bibb","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",260.16681034465813,"A","CEC Survey",2017,15,"I",272.31030553150225,"TON",8,{"v":1.0466758045377,"d":"1.05"},{"$f":"VLOOKUP(A61,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.7745695290000001,"d":"0.77"}]
["01009","01","AL","009","Blount","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",145.64035141548328,"A","CEC Survey",2017,15,"I",251.06085505647147,"TON",8,{"v":1.7238413160666182,"d":"1.72"},{"$f":"VLOOKUP(A62,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":1.2785294934855878,"d":"1.28"}]
["01009","01","AL","009","Blount","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.80867714179594,"A","CEC Survey",2017,15,"I",20.35628554511931,"TON",8,{"v":1.7238413160666186,"d":"1.72"},{"$f":"VLOOKUP(A63,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":1.2785294934855882,"d":"1.28"}]
["01009","01","AL","009","Blount","","2104008610","Hydronic heater: outdoor","Hydronic heater",141.70412570155128,"A","CEC Survey",2017,15,"I",244.2754265414317,"TON",8,{"v":1.7238413160666186,"d":"1.72"},{"$f":"VLOOKUP(A64,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":1.2785294934855882,"d":"1.28"}]
["01009","01","AL","009","Blount","","2104008620","Hydronic heater: indoor","Hydronic heater",90.53319142043556,"A","CEC Survey",2017,15,"I",156.0648558459147,"TON",8,{"v":1.7238413160666184,"d":"1.72"},{"$f":"VLOOKUP(A65,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":1.278529493485588,"d":"1.28"}]
["01009","01","AL","009","Blount","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.9362257139319805,"A","CEC Survey",2017,15,"I",6.7854285150397695,"TON",8,{"v":1.7238413160666184,"d":"1.72"},{"$f":"VLOOKUP(A66,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":1.278529493485588,"d":"1.28"}]
["01009","01","AL","009","Blount","","2104008100","Fireplace: general","Fireplace: general",1778.23815405,"A","CEC Survey",2017,15,"I",516.3992610960807,"TON",8,{"$f":"P67/J67","v":{"v":0.29039938206250004,"d":"0.29"}},{"$f":"VLOOKUP(A67,cordwood_density!A:D,4,FALSE)","v":1.3483},{"$f":"S67/T67","v":{"v":0.21538187500000003,"d":"0.22"}}]
["01009","01","AL","009","Blount","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",614.7058092709,"A","CEC Survey",2017,15,"I",317.3186693750224,"TON",8,{"v":0.5162122507861001,"d":"0.52"},{"$f":"VLOOKUP(A68,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.38286156700000007,"d":"0.38"}]
["01009","01","AL","009","Blount","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",812.9980058099,"A","CEC Survey",2017,15,"I",419.67953046373924,"TON",8,{"v":0.5162122507861,"d":"0.52"},{"$f":"VLOOKUP(A69,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.382861567,"d":"0.38"}]
["01009","01","AL","009","Blount","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",555.2181503092,"A","CEC Survey",2017,15,"I",286.61041104840734,"TON",8,{"v":0.5162122507861,"d":"0.52"},{"$f":"VLOOKUP(A70,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.382861567,"d":"0.38"}]
["01009","01","AL","009","Blount","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3257.0250966400004,"A","CEC Survey",2017,15,"I",648.3719246778107,"TON",8,{"v":0.1990687530614,"d":"0.20"},{"$f":"VLOOKUP(A71,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.147644258,"d":"0.15"}]
["01009","01","AL","009","Blount","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",838.8185938700001,"A","CEC Survey",2017,15,"I",251.70760627956093,"TON",8,{"v":0.300073947,"d":"0.30"},{"$f":"VLOOKUP(A72,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.22255725506192983,"d":"0.22"}]
["01009","01","AL","009","Blount","","2104009000","Wax Log; Total: All Combustor Types",null,173.38778630000002,"A","CEC Survey",2017,15,"I",59.54635071427613,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A73,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.2547124156345027,"d":"0.25"}]
["01009","01","AL","009","Blount","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",977.6182856424,"A","CEC Survey",2017,15,"I",1005.0612681810819,"TON",8,{"v":1.0280712655866997,"d":"1.03"},{"$f":"VLOOKUP(A74,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.7624944489999997,"d":"0.76"}]
["01009","01","AL","009","Blount","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1292.9790229464,"A","CEC Survey",2017,15,"I",1329.27458049756,"TON",8,{"v":1.0280712655867,"d":"1.03"},{"$f":"VLOOKUP(A75,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.762494449,"d":"0.76"}]
["01009","01","AL","009","Blount","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",883.0100644512,"A","CEC Survey",2017,15,"I",907.7972744861386,"TON",8,{"v":1.0280712655866997,"d":"1.03"},{"$f":"VLOOKUP(A76,cordwood_density!A:D,4,FALSE)","v":1.3483},{"v":0.7624944489999997,"d":"0.76"}]
["01011","01","AL","011","Bullock","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",15.111296649321462,"A","CEC Survey",2017,15,"I",22.93979981004486,"TON",8,{"v":1.5180563483329486,"d":"1.52"},{"$f":"VLOOKUP(A77,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":1.2202044436403412,"d":"1.22"}]
["01011","01","AL","011","Bullock","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.2252402688639024,"A","CEC Survey",2017,15,"I",1.8599837683820157,"TON",8,{"v":1.5180563483329486,"d":"1.52"},{"$f":"VLOOKUP(A78,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":1.2202044436403412,"d":"1.22"}]
["01011","01","AL","011","Bullock","","2104008610","Hydronic heater: outdoor","Hydronic heater",14.702883226366827,"A","CEC Survey",2017,15,"I",22.31980522058419,"TON",8,{"v":1.5180563483329488,"d":"1.52"},{"$f":"VLOOKUP(A79,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":1.2202044436403414,"d":"1.22"}]
["01011","01","AL","011","Bullock","","2104008620","Hydronic heater: indoor","Hydronic heater",9.393508727956585,"A","CEC Survey",2017,15,"I",14.259875557595455,"TON",8,{"v":1.5180563483329488,"d":"1.52"},{"$f":"VLOOKUP(A80,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":1.2202044436403414,"d":"1.22"}]
["01011","01","AL","011","Bullock","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.4084134229546341,"A","CEC Survey",2017,15,"I",0.619994589460672,"TON",8,{"v":1.5180563483329488,"d":"1.52"},{"$f":"VLOOKUP(A81,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":1.2202044436403414,"d":"1.22"}]
["01011","01","AL","011","Bullock","","2104008100","Fireplace: general","Fireplace: general",329.56061611,"A","CEC Survey",2017,15,"I",81.11772313952011,"TON",8,{"v":0.2461390080435,"d":"0.25"},{"$f":"VLOOKUP(A82,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.197845035,"d":"0.20"}]
["01011","01","AL","011","Bullock","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",105.7405411752,"A","CEC Survey",2017,15,"I",55.08354889050444,"TON",8,{"v":0.5209312178499,"d":"0.52"},{"$f":"VLOOKUP(A83,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.418721339,"d":"0.42"}]
["01011","01","AL","011","Bullock","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",139.8503931672,"A","CEC Survey",2017,15,"I",72.85243562937683,"TON",8,{"v":0.5209312178499,"d":"0.52"},{"$f":"VLOOKUP(A84,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.418721339,"d":"0.42"}]
["01011","01","AL","011","Bullock","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",95.50758557760001,"A","CEC Survey",2017,15,"I",49.752882868842725,"TON",8,{"v":0.5209312178499,"d":"0.52"},{"$f":"VLOOKUP(A85,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.418721339,"d":"0.42"}]
["01011","01","AL","011","Bullock","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,485.97474996,"A","CEC Survey",2017,15,"I",88.00344274713231,"TON",8,{"v":0.18108645100259996,"d":"0.18"},{"$f":"VLOOKUP(A86,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.14555618599999998,"d":"0.15"}]
["01011","01","AL","011","Bullock","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",106.69118656,"A","CEC Survey",2017,15,"I",25.620833489931297,"TON",8,{"v":0.24014011200000002,"d":"0.24"},{"$f":"VLOOKUP(A87,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.19302315891005548,"d":"0.19"}]
["01011","01","AL","011","Bullock","","2104009000","Wax Log; Total: All Combustor Types",null,52.71210788831852,"A","CEC Survey",2017,15,"I",12.341607057740157,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A88,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.18819411622859897,"d":"0.19"}]
["01011","01","AL","011","Bullock","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",127.85871022539999,"A","CEC Survey",2017,15,"I",118.30671455232171,"TON",8,{"v":0.925292569773,"d":"0.93"},{"$f":"VLOOKUP(A89,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.7437445300000001,"d":"0.74"}]
["01011","01","AL","011","Bullock","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",169.10345545939998,"A","CEC Survey",2017,15,"I",156.47017085952226,"TON",8,{"v":0.925292569773,"d":"0.93"},{"$f":"VLOOKUP(A90,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.7437445300000001,"d":"0.74"}]
["01011","01","AL","011","Bullock","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",115.4852866552,"A","CEC Survey",2017,15,"I",106.85767766016156,"TON",8,{"v":0.925292569773,"d":"0.93"},{"$f":"VLOOKUP(A91,cordwood_density!A:D,4,FALSE)","v":1.2441},{"v":0.7437445300000001,"d":"0.74"}]
["01013","01","AL","013","Butler","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",31.989761364083495,"A","CEC Survey",2017,15,"I",47.86943700430542,"TON",8,{"v":1.4963986901775024,"d":"1.50"},{"$f":"VLOOKUP(A92,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":1.1802182271295074,"d":"1.18"}]
["01013","01","AL","013","Butler","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.593764434925689,"A","CEC Survey",2017,15,"I",3.881305703051791,"TON",8,{"v":1.4963986901775024,"d":"1.50"},{"$f":"VLOOKUP(A93,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":1.1802182271295074,"d":"1.18"}]
["01013","01","AL","013","Butler","","2104008610","Hydronic heater: outdoor","Hydronic heater",31.125173219108266,"A","CEC Survey",2017,15,"I",46.575668436621484,"TON",8,{"v":1.4963986901775024,"d":"1.50"},{"$f":"VLOOKUP(A94,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":1.1802182271295074,"d":"1.18"}]
["01013","01","AL","013","Butler","","2104008620","Hydronic heater: indoor","Hydronic heater",19.885527334430282,"A","CEC Survey",2017,15,"I",29.756677056730396,"TON",8,{"v":1.4963986901775024,"d":"1.50"},{"$f":"VLOOKUP(A95,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":1.1802182271295074,"d":"1.18"}]
["01013","01","AL","013","Butler","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8645881449752296,"A","CEC Survey",2017,15,"I",1.2937685676839303,"TON",8,{"v":1.4963986901775026,"d":"1.50"},{"$f":"VLOOKUP(A96,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":1.1802182271295074,"d":"1.18"}]
["01013","01","AL","013","Butler","","2104008100","Fireplace: general","Fireplace: general",786.3350463,"A","CEC Survey",2017,15,"I",203.768680600081,"TON",8,{"v":0.25913722345060003,"d":"0.26"},{"$f":"VLOOKUP(A97,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.20438301400000003,"d":"0.20"}]
["01013","01","AL","013","Butler","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",208.1821693965,"A","CEC Survey",2017,15,"I",127.83201700710887,"TON",8,{"v":0.6140392204466,"d":"0.61"},{"$f":"VLOOKUP(A98,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.484296254,"d":"0.48"}]
["01013","01","AL","013","Butler","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",275.3377079115,"A","CEC Survey",2017,15,"I",169.06815152553108,"TON",8,{"v":0.6140392204465999,"d":"0.61"},{"$f":"VLOOKUP(A99,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.48429625399999987,"d":"0.48"}]
["01013","01","AL","013","Butler","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",188.03550784200002,"A","CEC Survey",2017,15,"I",115.46117665158222,"TON",8,{"v":0.6140392204466,"d":"0.61"},{"$f":"VLOOKUP(A100,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.484296254,"d":"0.48"}]
["01013","01","AL","013","Butler","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1004.2319413499999,"A","CEC Survey",2017,15,"I",186.33122984791336,"TON",8,{"v":0.18554601001579998,"d":"0.19"},{"$f":"VLOOKUP(A101,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.14634120199999998,"d":"0.15"}]
["01013","01","AL","013","Butler","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",229.45379085000002,"A","CEC Survey",2017,15,"I",55.82706757791971,"TON",8,{"v":0.243304185,"d":"0.24"},{"$f":"VLOOKUP(A102,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.19189540578910008,"d":"0.19"}]
["01013","01","AL","013","Butler","","2104009000","Wax Log; Total: All Combustor Types",null,101.2589538454075,"A","CEC Survey",2017,15,"I",23.7079917594191,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A103,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.1846614874990141,"d":"0.18"}]
["01013","01","AL","013","Butler","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",249.341347773,"A","CEC Survey",2017,15,"I",235.98320873087874,"TON",8,{"v":0.9464262980791999,"d":"0.95"},{"$f":"VLOOKUP(A104,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.7464518479999999,"d":"0.75"}]
["01013","01","AL","013","Butler","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",329.77404060299995,"A","CEC Survey",2017,15,"I",312.106824450517,"TON",8,{"v":0.9464262980792,"d":"0.95"},{"$f":"VLOOKUP(A105,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.746451848,"d":"0.75"}]
["01013","01","AL","013","Butler","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",225.21153992400002,"A","CEC Survey",2017,15,"I",213.14612401498727,"TON",8,{"v":0.9464262980791999,"d":"0.95"},{"$f":"VLOOKUP(A106,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.7464518479999999,"d":"0.75"}]
["01015","01","AL","015","Calhoun","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",172.24397233496387,"A","CEC Survey",2017,15,"I",272.15565166892156,"TON",8,{"v":1.5800590753890584,"d":"1.58"},{"$f":"VLOOKUP(A107,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":1.1809111176300884,"d":"1.18"}]
["01015","01","AL","015","Calhoun","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.965727486618693,"A","CEC Survey",2017,15,"I",22.066674459642286,"TON",8,{"v":1.580059075389058,"d":"1.58"},{"$f":"VLOOKUP(A108,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":1.1809111176300882,"d":"1.18"}]
["01015","01","AL","015","Calhoun","","2104008610","Hydronic heater: outdoor","Hydronic heater",167.5887298394243,"A","CEC Survey",2017,15,"I",264.80009351570743,"TON",8,{"v":1.5800590753890582,"d":"1.58"},{"$f":"VLOOKUP(A109,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":1.1809111176300884,"d":"1.18"}]
["01015","01","AL","015","Calhoun","","2104008620","Hydronic heater: indoor","Hydronic heater",107.07057739740999,"A","CEC Survey",2017,15,"I",169.1778375239242,"TON",8,{"v":1.580059075389058,"d":"1.58"},{"$f":"VLOOKUP(A110,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":1.1809111176300882,"d":"1.18"}]
["01015","01","AL","015","Calhoun","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.655242495539564,"A","CEC Survey",2017,15,"I",7.355558153214096,"TON",8,{"v":1.5800590753890582,"d":"1.58"},{"$f":"VLOOKUP(A111,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":1.1809111176300884,"d":"1.18"}]
["01015","01","AL","015","Calhoun","","2104008100","Fireplace: general","Fireplace: general",6263.6876330939995,"A","CEC Survey",2017,15,"I",1481.327916710564,"TON",8,{"v":0.236494538598,"d":"0.24"},{"$f":"VLOOKUP(A112,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.176752271,"d":"0.18"}]
["01015","01","AL","015","Calhoun","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1098.27010346904,"A","CEC Survey",2017,15,"I",652.5367661644792,"TON",8,{"v":0.594149621394,"d":"0.59"},{"$f":"VLOOKUP(A113,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.4440580129999999,"d":"0.44"}]
["01015","01","AL","015","Calhoun","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1452.55078200744,"A","CEC Survey",2017,15,"I",863.032497185279,"TON",8,{"v":0.594149621394,"d":"0.59"},{"$f":"VLOOKUP(A114,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.4440580129999999,"d":"0.44"}]
["01015","01","AL","015","Calhoun","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",991.9858999075201,"A","CEC Survey",2017,15,"I",589.3880468582394,"TON",8,{"v":0.594149621394,"d":"0.59"},{"$f":"VLOOKUP(A115,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.4440580129999999,"d":"0.44"}]
["01015","01","AL","015","Calhoun","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,6521.407582356001,"A","CEC Survey",2017,15,"I",1290.2989339842181,"TON",8,{"v":0.19785589501800002,"d":"0.20"},{"$f":"VLOOKUP(A116,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.147874361,"d":"0.15"}]
["01015","01","AL","015","Calhoun","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1347.75745758,"A","CEC Survey",2017,15,"I",300.6653363367646,"TON",8,{"v":0.223085641,"d":"0.22"},{"$f":"VLOOKUP(A117,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.16673067339312406,"d":"0.17"}]
["01015","01","AL","015","Calhoun","","2104009000","Wax Log; Total: All Combustor Types",null,647.7556821948983,"A","CEC Survey",2017,15,"I",222.4579242415912,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A118,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.2566732062780269,"d":"0.26"}]
["01015","01","AL","015","Calhoun","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1278.51728172993,"A","CEC Survey",2017,15,"I",1110.8026780657942,"TON",8,{"v":0.8688210116040002,"d":"0.87"},{"$f":"VLOOKUP(A119,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.649343058,"d":"0.65"}]
["01015","01","AL","015","Calhoun","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1690.9422113202297,"A","CEC Survey",2017,15,"I",1469.126122603147,"TON",8,{"v":0.8688210116040002,"d":"0.87"},{"$f":"VLOOKUP(A120,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.649343058,"d":"0.65"}]
["01015","01","AL","015","Calhoun","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1154.78980285284,"A","CEC Survey",2017,15,"I",1003.3056447045884,"TON",8,{"v":0.8688210116040002,"d":"0.87"},{"$f":"VLOOKUP(A121,cordwood_density!A:D,4,FALSE)","v":1.338},{"v":0.649343058,"d":"0.65"}]
["01017","01","AL","017","Chambers","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",65.43709027301207,"A","CEC Survey",2017,15,"I",95.68423500265924,"TON",8,{"v":1.4622324220629634,"d":"1.46"},{"$f":"VLOOKUP(A122,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":1.2097562853172528,"d":"1.21"}]
["01017","01","AL","017","Chambers","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.305710022136114,"A","CEC Survey",2017,15,"I",7.75818121643183,"TON",8,{"v":1.4622324220629637,"d":"1.46"},{"$f":"VLOOKUP(A123,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":1.2097562853172528,"d":"1.21"}]
["01017","01","AL","017","Chambers","","2104008610","Hydronic heater: outdoor","Hydronic heater",63.66852026563336,"A","CEC Survey",2017,15,"I",93.09817459718195,"TON",8,{"v":1.4622324220629637,"d":"1.46"},{"$f":"VLOOKUP(A124,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":1.2097562853172528,"d":"1.21"}]
["01017","01","AL","017","Chambers","","2104008620","Hydronic heater: indoor","Hydronic heater",40.67711016971021,"A","CEC Survey",2017,15,"I",59.479389325977365,"TON",8,{"v":1.4622324220629634,"d":"1.46"},{"$f":"VLOOKUP(A125,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":1.2097562853172528,"d":"1.21"}]
["01017","01","AL","017","Chambers","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.7685700073787047,"A","CEC Survey",2017,15,"I",2.586060405477277,"TON",8,{"v":1.4622324220629637,"d":"1.46"},{"$f":"VLOOKUP(A126,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":1.2097562853172528,"d":"1.21"}]
["01017","01","AL","017","Chambers","","2104008100","Fireplace: general","Fireplace: general",1636.185919158,"A","CEC Survey",2017,15,"I",374.71823157118274,"TON",8,{"v":0.22901934748590005,"d":"0.23"},{"$f":"VLOOKUP(A127,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.18947575700000002,"d":"0.19"}]
["01017","01","AL","017","Chambers","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",398.23655368402,"A","CEC Survey",2017,15,"I",224.8373258767779,"TON",8,{"v":0.5645823413166,"d":"0.56"},{"$f":"VLOOKUP(A128,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.46709881799999997,"d":"0.47"}]
["01017","01","AL","017","Chambers","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",526.69995809822,"A","CEC Survey",2017,15,"I",297.3654955144482,"TON",8,{"v":0.5645823413166,"d":"0.56"},{"$f":"VLOOKUP(A129,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.46709881799999997,"d":"0.47"}]
["01017","01","AL","017","Chambers","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",359.69753235976003,"A","CEC Survey",2017,15,"I",203.07887498547683,"TON",8,{"v":0.5645823413166,"d":"0.56"},{"$f":"VLOOKUP(A130,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.46709881799999997,"d":"0.47"}]
["01017","01","AL","017","Chambers","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2071.440547872,"A","CEC Survey",2017,15,"I",368.0149610647853,"TON",8,{"$f":"P131/J131","v":{"v":0.17766136780650002,"d":"0.18"}},{"$f":"VLOOKUP(A131,cordwood_density!A:D,4,FALSE)","v":1.2087},{"$f":"S131/T131","v":{"v":0.146985495,"d":"0.15"}}]
["01017","01","AL","017","Chambers","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",456.397178746,"A","CEC Survey",2017,15,"I",114.96633613961706,"TON",8,{"v":0.251899752,"d":"0.25"},{"$f":"VLOOKUP(A132,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.20840551998014392,"d":"0.21"}]
["01017","01","AL","017","Chambers","","2104009000","Wax Log; Total: All Combustor Types",null,196.68654098709368,"A","CEC Survey",2017,15,"I",67.54781291302135,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A133,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.28413067758749067,"d":"0.28"}]
["01017","01","AL","017","Chambers","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",485.91359937056,"A","CEC Survey",2017,15,"I",410.83810274414833,"TON",8,{"v":0.8454962019510001,"d":"0.85"},{"$f":"VLOOKUP(A134,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.69950873,"d":"0.70"}]
["01017","01","AL","017","Chambers","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",642.65992174816,"A","CEC Survey",2017,15,"I",543.3665229841962,"TON",8,{"v":0.8454962019510002,"d":"0.85"},{"$f":"VLOOKUP(A135,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.6995087300000001,"d":"0.70"}]
["01017","01","AL","017","Chambers","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",438.88970265728005,"A","CEC Survey",2017,15,"I",371.079576672134,"TON",8,{"v":0.8454962019510001,"d":"0.85"},{"$f":"VLOOKUP(A136,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.69950873,"d":"0.70"}]
["01019","01","AL","019","Cherokee","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",62.3012285470037,"A","CEC Survey",2017,15,"I",106.36927989426923,"TON",8,{"v":1.7073384004621674,"d":"1.71"},{"$f":"VLOOKUP(A137,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":1.2580785501894978,"d":"1.26"}]
["01019","01","AL","019","Cherokee","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.051450963270571,"A","CEC Survey",2017,15,"I",8.62453620764345,"TON",8,{"v":1.7073384004621672,"d":"1.71"},{"$f":"VLOOKUP(A138,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":1.2580785501894975,"d":"1.26"}]
["01019","01","AL","019","Cherokee","","2104008610","Hydronic heater: outdoor","Hydronic heater",60.61741155924685,"A","CEC Survey",2017,15,"I",103.4944344917214,"TON",8,{"v":1.7073384004621674,"d":"1.71"},{"$f":"VLOOKUP(A139,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":1.2580785501894978,"d":"1.26"}]
["01019","01","AL","019","Cherokee","","2104008620","Hydronic heater: indoor","Hydronic heater",38.72779071840771,"A","CEC Survey",2017,15,"I",66.1214442585998,"TON",8,{"v":1.7073384004621674,"d":"1.71"},{"$f":"VLOOKUP(A140,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":1.2580785501894978,"d":"1.26"}]
["01019","01","AL","019","Cherokee","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.683816987756857,"A","CEC Survey",2017,15,"I",2.874845402547817,"TON",8,{"v":1.7073384004621672,"d":"1.71"},{"$f":"VLOOKUP(A141,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":1.2580785501894975,"d":"1.26"}]
["01019","01","AL","019","Cherokee","","2104008100","Fireplace: general","Fireplace: general",839.4964706100001,"A","CEC Survey",2017,15,"I",248.3582109776511,"TON",8,{"v":0.2958418762585,"d":"0.30"},{"$f":"VLOOKUP(A142,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.217995635,"d":"0.22"}]
["01019","01","AL","019","Cherokee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",305.2761264544,"A","CEC Survey",2017,15,"I",146.57996041842108,"TON",8,{"v":0.4801553338639999,"d":"0.48"},{"$f":"VLOOKUP(A143,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.35380983999999993,"d":"0.35"}]
["01019","01","AL","019","Cherokee","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",403.75229627839997,"A","CEC Survey",2017,15,"I",193.86381861791176,"TON",8,{"v":0.48015533386399994,"d":"0.48"},{"$f":"VLOOKUP(A144,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.35380984,"d":"0.35"}]
["01019","01","AL","019","Cherokee","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",275.7332755072,"A","CEC Survey",2017,15,"I",132.3948029585739,"TON",8,{"v":0.480155333864,"d":"0.48"},{"$f":"VLOOKUP(A145,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.35380984,"d":"0.35"}]
["01019","01","AL","019","Cherokee","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1618.0217125149998,"A","CEC Survey",2017,15,"I",323.94006113829374,"TON",8,{"v":0.2002074871015,"d":"0.20"},{"$f":"VLOOKUP(A146,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.147525965,"d":"0.15"}]
["01019","01","AL","019","Cherokee","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",411.43163776500006,"A","CEC Survey",2017,15,"I",102.7072205467604,"TON",8,{"v":0.249633745,"d":"0.25"},{"$f":"VLOOKUP(A147,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.18394646304620146,"d":"0.18"}]
["01019","01","AL","019","Cherokee","","2104009000","Wax Log; Total: All Combustor Types",null,155.04828464697505,"A","CEC Survey",2017,15,"I",53.24803858595483,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A148,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.2530607545501437,"d":"0.25"}]
["01019","01","AL","019","Cherokee","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",465.84228110885005,"A","CEC Survey",2017,15,"I",474.54355371060353,"TON",8,{"v":1.0186785806154,"d":"1.02"},{"$f":"VLOOKUP(A149,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.750628974,"d":"0.75"}]
["01019","01","AL","019","Cherokee","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",616.1139846923501,"A","CEC Survey",2017,15,"I",627.6221194237014,"TON",8,{"v":1.0186785806154,"d":"1.02"},{"$f":"VLOOKUP(A150,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.750628974,"d":"0.75"}]
["01019","01","AL","019","Cherokee","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",420.7607700338001,"A","CEC Survey",2017,15,"I",428.6199839966742,"TON",8,{"v":1.0186785806154,"d":"1.02"},{"$f":"VLOOKUP(A151,cordwood_density!A:D,4,FALSE)","v":1.3571},{"v":0.750628974,"d":"0.75"}]
["01021","01","AL","021","Chilton","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",99.65606834076117,"A","CEC Survey",2017,15,"I",162.15229014768028,"TON",8,{"v":1.6271190791234236,"d":"1.63"},{"$f":"VLOOKUP(A152,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":1.2683132583392498,"d":"1.27"}]
["01021","01","AL","021","Chilton","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.080221757359013,"A","CEC Survey",2017,15,"I",13.147482984947048,"TON",8,{"v":1.6271190791234236,"d":"1.63"},{"$f":"VLOOKUP(A153,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":1.2683132583392498,"d":"1.27"}]
["01021","01","AL","021","Chilton","","2104008610","Hydronic heater: outdoor","Hydronic heater",96.96266108830817,"A","CEC Survey",2017,15,"I",157.7697958193646,"TON",8,{"v":1.6271190791234234,"d":"1.63"},{"$f":"VLOOKUP(A154,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":1.2683132583392498,"d":"1.27"}]
["01021","01","AL","021","Chilton","","2104008620","Hydronic heater: indoor","Hydronic heater",61.94836680641911,"A","CEC Survey",2017,15,"I",100.79736955126072,"TON",8,{"v":1.6271190791234236,"d":"1.63"},{"$f":"VLOOKUP(A155,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":1.2683132583392498,"d":"1.27"}]
["01021","01","AL","021","Chilton","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.693407252453005,"A","CEC Survey",2017,15,"I",4.382494328315683,"TON",8,{"v":1.6271190791234236,"d":"1.63"},{"$f":"VLOOKUP(A156,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":1.2683132583392498,"d":"1.27"}]
["01021","01","AL","021","Chilton","","2104008100","Fireplace: general","Fireplace: general",1470.09868416,"A","CEC Survey",2017,15,"I",398.4846304950241,"TON",8,{"v":0.2710597831211,"d":"0.27"},{"$f":"VLOOKUP(A157,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.21128675900000002,"d":"0.21"}]
["01021","01","AL","021","Chilton","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",505.86815811968,"A","CEC Survey",2017,15,"I",264.69002313707404,"TON",8,{"v":0.5232391461857,"d":"0.52"},{"$f":"VLOOKUP(A158,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.407856533,"d":"0.41"}]
["01021","01","AL","021","Chilton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",669.05143493248,"A","CEC Survey",2017,15,"I",350.07390156838824,"TON",8,{"v":0.5232391461857,"d":"0.52"},{"$f":"VLOOKUP(A159,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.407856533,"d":"0.41"}]
["01021","01","AL","021","Chilton","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",456.91317507584006,"A","CEC Survey",2017,15,"I",239.07485960767983,"TON",8,{"v":0.5232391461857,"d":"0.52"},{"$f":"VLOOKUP(A160,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.407856533,"d":"0.41"}]
["01021","01","AL","021","Chilton","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2444.667554304,"A","CEC Survey",2017,15,"I",460.7715934399287,"TON",8,{"v":0.1884802670321,"d":"0.19"},{"$f":"VLOOKUP(A161,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.146917349,"d":"0.15"}]
["01021","01","AL","021","Chilton","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",595.43109312,"A","CEC Survey",2017,15,"I",173.96047949682162,"TON",8,{"v":0.292158877,"d":"0.29"},{"$f":"VLOOKUP(A162,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.22773316470496532,"d":"0.23"}]
["01021","01","AL","021","Chilton","","2104009000","Wax Log; Total: All Combustor Types",null,140.52036736,"A","CEC Survey",2017,15,"I",48.258734111985596,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A163,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.2676972094473459,"d":"0.27"}]
["01021","01","AL","021","Chilton","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",727.5845049843199,"A","CEC Survey",2017,15,"I",722.6866101046213,"TON",8,{"v":0.9932682803905999,"d":"0.99"},{"$f":"VLOOKUP(A164,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.7742367139999999,"d":"0.77"}]
["01021","01","AL","021","Chilton","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",962.2891840115199,"A","CEC Survey",2017,15,"I",955.8113230415959,"TON",8,{"v":0.9932682803905999,"d":"0.99"},{"$f":"VLOOKUP(A165,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.7742367139999999,"d":"0.77"}]
["01021","01","AL","021","Chilton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",657.17310127616,"A","CEC Survey",2017,15,"I",652.749196223529,"TON",8,{"v":0.9932682803906,"d":"0.99"},{"$f":"VLOOKUP(A166,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.774236714,"d":"0.77"}]
["01023","01","AL","023","Choctaw","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",33.92729972926825,"A","CEC Survey",2017,15,"I",54.053850888278156,"TON",8,{"v":1.5932258481993846,"d":"1.59"},{"$f":"VLOOKUP(A167,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":1.24286281940821,"d":"1.24"}]
["01023","01","AL","023","Choctaw","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.7508621402109394,"A","CEC Survey",2017,15,"I",4.382744666617148,"TON",8,{"v":1.5932258481993844,"d":"1.59"},{"$f":"VLOOKUP(A168,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":1.2428628194082099,"d":"1.24"}]
["01023","01","AL","023","Choctaw","","2104008610","Hydronic heater: outdoor","Hydronic heater",33.01034568253127,"A","CEC Survey",2017,15,"I",52.59293599940577,"TON",8,{"v":1.5932258481993842,"d":"1.59"},{"$f":"VLOOKUP(A169,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":1.2428628194082099,"d":"1.24"}]
["01023","01","AL","023","Choctaw","","2104008620","Hydronic heater: indoor","Hydronic heater",21.089943074950536,"A","CEC Survey",2017,15,"I",33.6010424440648,"TON",8,{"v":1.5932258481993844,"d":"1.59"},{"$f":"VLOOKUP(A170,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":1.2428628194082099,"d":"1.24"}]
["01023","01","AL","023","Choctaw","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9169540467369798,"A","CEC Survey",2017,15,"I",1.4609148888723826,"TON",8,{"v":1.5932258481993844,"d":"1.59"},{"$f":"VLOOKUP(A171,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":1.2428628194082099,"d":"1.24"}]
["01023","01","AL","023","Choctaw","","2104008100","Fireplace: general","Fireplace: general",576.421293933,"A","CEC Survey",2017,15,"I",159.9409787252476,"TON",8,{"v":0.2774723633715,"d":"0.28"},{"$f":"VLOOKUP(A172,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.216453985,"d":"0.22"}]
["01023","01","AL","023","Choctaw","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",197.48626245306,"A","CEC Survey",2017,15,"I",128.51997118426456,"TON",8,{"v":0.6507792976983001,"d":"0.65"},{"$f":"VLOOKUP(A173,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.5076677570000001,"d":"0.51"}]
["01023","01","AL","023","Choctaw","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",261.19150840566,"A","CEC Survey",2017,15,"I",169.97802640499503,"TON",8,{"v":0.6507792976983,"d":"0.65"},{"$f":"VLOOKUP(A174,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.507667757,"d":"0.51"}]
["01023","01","AL","023","Choctaw","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",178.37468866728003,"A","CEC Survey",2017,15,"I",116.0825546180454,"TON",8,{"v":0.6507792976983,"d":"0.65"},{"$f":"VLOOKUP(A175,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.507667757,"d":"0.51"}]
["01023","01","AL","023","Choctaw","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,852.383897631,"A","CEC Survey",2017,15,"I",161.72505674854432,"TON",8,{"v":0.18973265121270003,"d":"0.19"},{"$f":"VLOOKUP(A176,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.148008933,"d":"0.15"}]
["01023","01","AL","023","Choctaw","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",211.41303033600002,"A","CEC Survey",2017,15,"I",63.651249566015466,"TON",8,{"v":0.301075338,"d":"0.30"},{"$f":"VLOOKUP(A177,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.23486647788439038,"d":"0.23"}]
["01023","01","AL","023","Choctaw","","2104009000","Wax Log; Total: All Combustor Types",null,78.46491700105832,"A","CEC Survey",2017,15,"I",18.371171486766887,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A178,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.18264474608003742,"d":"0.18"}]
["01023","01","AL","023","Choctaw","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",257.77279742255996,"A","CEC Survey",2017,15,"I",263.8407364465788,"TON",8,{"v":1.0235398734261,"d":"1.02"},{"$f":"VLOOKUP(A179,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.798455319,"d":"0.80"}]
["01023","01","AL","023","Choctaw","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",340.92531272016,"A","CEC Survey",2017,15,"I",348.9506514293461,"TON",8,{"v":1.0235398734261,"d":"1.02"},{"$f":"VLOOKUP(A180,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.798455319,"d":"0.80"}]
["01023","01","AL","023","Choctaw","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",232.82704283328002,"A","CEC Survey",2017,15,"I",238.3077619517486,"TON",8,{"v":1.0235398734261,"d":"1.02"},{"$f":"VLOOKUP(A181,cordwood_density!A:D,4,FALSE)","v":1.2819},{"v":0.798455319,"d":"0.80"}]
["01025","01","AL","025","Clarke","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",46.87726036365184,"A","CEC Survey",2017,15,"I",71.04416016464867,"TON",8,{"v":1.5155356693953814,"d":"1.52"},{"$f":"VLOOKUP(A182,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":1.184197272538976,"d":"1.18"}]
["01025","01","AL","025","Clarke","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.8008589484042035,"A","CEC Survey",2017,15,"I",5.76033731064719,"TON",8,{"v":1.5155356693953812,"d":"1.52"},{"$f":"VLOOKUP(A183,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":1.1841972725389758,"d":"1.18"}]
["01025","01","AL","025","Clarke","","2104008610","Hydronic heater: outdoor","Hydronic heater",45.61030738085044,"A","CEC Survey",2017,15,"I",69.12404772776627,"TON",8,{"v":1.5155356693953812,"d":"1.52"},{"$f":"VLOOKUP(A184,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":1.1841972725389758,"d":"1.18"}]
["01025","01","AL","025","Clarke","","2104008620","Hydronic heater: indoor","Hydronic heater",29.13991860443223,"A","CEC Survey",2017,15,"I",44.162586048295125,"TON",8,{"v":1.5155356693953814,"d":"1.52"},{"$f":"VLOOKUP(A185,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":1.184197272538976,"d":"1.18"}]
["01025","01","AL","025","Clarke","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2669529828014012,"A","CEC Survey",2017,15,"I",1.9201124368823967,"TON",8,{"v":1.5155356693953814,"d":"1.52"},{"$f":"VLOOKUP(A186,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":1.184197272538976,"d":"1.18"}]
["01025","01","AL","025","Clarke","","2104008100","Fireplace: general","Fireplace: general",1252.417570110433,"A","CEC Survey",2017,15,"I",327.1870787860756,"TON",8,{"v":0.26124440170319996,"d":"0.26"},{"$f":"VLOOKUP(A187,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.20412908399999996,"d":"0.20"}]
["01025","01","AL","025","Clarke","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",289.1718850325758,"A","CEC Survey",2017,15,"I",186.98284676861476,"TON",8,{"v":0.6466148904743999,"d":"0.65"},{"$f":"VLOOKUP(A188,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.5052468279999999,"d":"0.51"}]
["01025","01","AL","025","Clarke","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",382.45313826889054,"A","CEC Survey",2017,15,"I",247.2998941133292,"TON",8,{"v":0.6466148904744,"d":"0.65"},{"$f":"VLOOKUP(A189,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.505246828,"d":"0.51"}]
["01025","01","AL","025","Clarke","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",261.1875090616814,"A","CEC Survey",2017,15,"I",168.88773256520045,"TON",8,{"v":0.6466148904743999,"d":"0.65"},{"$f":"VLOOKUP(A190,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.5052468279999999,"d":"0.51"}]
["01025","01","AL","025","Clarke","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1438.8540733778493,"A","CEC Survey",2017,15,"I",271.9451031437938,"TON",8,{"v":0.18900116987219998,"d":"0.19"},{"$f":"VLOOKUP(A191,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.14768023899999996,"d":"0.15"}]
["01025","01","AL","025","Clarke","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",333.313861158713,"A","CEC Survey",2017,15,"I",81.50700603254582,"TON",8,{"v":0.244535303,"d":"0.24"},{"$f":"VLOOKUP(A192,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.19107306063447413,"d":"0.19"}]
["01025","01","AL","025","Clarke","","2104009000","Wax Log; Total: All Combustor Types",null,137.91325885459034,"A","CEC Survey",2017,15,"I",32.2899484961206,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A193,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.18294444444444444,"d":"0.18"}]
["01025","01","AL","025","Clarke","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",347.5595514021566,"A","CEC Survey",2017,15,"I",336.10936170950316,"TON",8,{"v":0.967055459571,"d":"0.97"},{"$f":"VLOOKUP(A194,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.755630145,"d":"0.76"}]
["01025","01","AL","025","Clarke","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",459.6755357254329,"A","CEC Survey",2017,15,"I",444.5317364545042,"TON",8,{"$f":"P195/J195","v":{"v":0.9670554595710001,"d":"0.97"}},{"$f":"VLOOKUP(A195,cordwood_density!A:D,4,FALSE)","v":1.2798},{"$f":"S195/T195","v":{"v":0.755630145,"d":"0.76"}}]
["01025","01","AL","025","Clarke","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",313.92475610517374,"A","CEC Survey",2017,15,"I",303.5826492860029,"TON",8,{"v":0.967055459571,"d":"0.97"},{"$f":"VLOOKUP(A196,cordwood_density!A:D,4,FALSE)","v":1.2798},{"v":0.755630145,"d":"0.76"}]
["01027","01","AL","027","Clay","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",40.72583003152387,"A","CEC Survey",2017,15,"I",63.230215892220166,"TON",8,{"v":1.5525826200049637,"d":"1.55"},{"$f":"VLOOKUP(A197,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":1.2056084951117905,"d":"1.21"}]
["01027","01","AL","027","Clay","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.3020943268803133,"A","CEC Survey",2017,15,"I",5.126774261531365,"TON",8,{"v":1.552582620004964,"d":"1.55"},{"$f":"VLOOKUP(A198,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":1.2056084951117905,"d":"1.21"}]
["01027","01","AL","027","Clay","","2104008610","Hydronic heater: outdoor","Hydronic heater",39.62513192256376,"A","CEC Survey",2017,15,"I",61.52129113837638,"TON",8,{"v":1.552582620004964,"d":"1.55"},{"$f":"VLOOKUP(A199,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":1.2056084951117905,"d":"1.21"}]
["01027","01","AL","027","Clay","","2104008620","Hydronic heater: indoor","Hydronic heater",25.316056506082404,"A","CEC Survey",2017,15,"I",39.30526933840713,"TON",8,{"v":1.5525826200049637,"d":"1.55"},{"$f":"VLOOKUP(A200,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":1.2056084951117905,"d":"1.21"}]
["01027","01","AL","027","Clay","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.1006981089601044,"A","CEC Survey",2017,15,"I",1.7089247538437884,"TON",8,{"v":1.5525826200049642,"d":"1.55"},{"$f":"VLOOKUP(A201,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":1.2056084951117907,"d":"1.21"}]
["01027","01","AL","027","Clay","","2104008100","Fireplace: general","Fireplace: general",686.7585965606547,"A","CEC Survey",2017,15,"I",191.4234118861092,"TON",8,{"v":0.2787346424854001,"d":"0.28"},{"$f":"VLOOKUP(A202,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.21644249300000007,"d":"0.22"}]
["01027","01","AL","027","Clay","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",162.78622401223575,"A","CEC Survey",2017,15,"I",105.30472403868596,"TON",8,{"v":0.6468896534559999,"d":"0.65"},{"$f":"VLOOKUP(A203,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.50232152,"d":"0.50"}]
["01027","01","AL","027","Clay","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",215.2979091774731,"A","CEC Survey",2017,15,"I",139.2739898576169,"TON",8,{"v":0.6468896534559998,"d":"0.65"},{"$f":"VLOOKUP(A204,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.5023215199999999,"d":"0.50"}]
["01027","01","AL","027","Clay","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",147.03271846266455,"A","CEC Survey",2017,15,"I",95.11394429300668,"TON",8,{"v":0.646889653456,"d":"0.65"},{"$f":"VLOOKUP(A205,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.50232152,"d":"0.50"}]
["01027","01","AL","027","Clay","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,876.680809250234,"A","CEC Survey",2017,15,"I",165.11104287685467,"TON",8,{"v":0.18833655434760002,"d":"0.19"},{"$f":"VLOOKUP(A206,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.146246742,"d":"0.15"}]
["01027","01","AL","027","Clay","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",222.64772381771,"A","CEC Survey",2017,15,"I",69.62933536487638,"TON",8,{"v":0.312733201,"d":"0.31"},{"$f":"VLOOKUP(A207,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.24284298881813945,"d":"0.24"}]
["01027","01","AL","027","Clay","","2104009000","Wax Log; Total: All Combustor Types",null,76.66954549333961,"A","CEC Survey",2017,15,"I",26.330526171845758,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A208,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.2666786379872651,"d":"0.27"}]
["01027","01","AL","027","Clay","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",241.07197275858147,"A","CEC Survey",2017,15,"I",250.97438169383204,"TON",8,{"v":1.0410765665620003,"d":"1.04"},{"$f":"VLOOKUP(A209,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.8084147900000002,"d":"0.81"}]
["01027","01","AL","027","Clay","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",318.8371252613497,"A","CEC Survey",2017,15,"I",331.9338596595843,"TON",8,{"v":1.041076566562,"d":"1.04"},{"$f":"VLOOKUP(A210,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.80841479,"d":"0.81"}]
["01027","01","AL","027","Clay","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",217.74242700775102,"A","CEC Survey",2017,15,"I",226.6865383041064,"TON",8,{"v":1.0410765665620003,"d":"1.04"},{"$f":"VLOOKUP(A211,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":0.8084147900000002,"d":"0.81"}]
["01029","01","AL","029","Cleburne","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",44.58665200939928,"A","CEC Survey",2017,15,"I",69.27047027666845,"TON",8,{"v":1.5536145271025417,"d":"1.55"},{"$f":"VLOOKUP(A212,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":1.2685674263922118,"d":"1.27"}]
["01029","01","AL","029","Cleburne","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.6151339467080494,"A","CEC Survey",2017,15,"I",5.616524617027172,"TON",8,{"v":1.5536145271025417,"d":"1.55"},{"$f":"VLOOKUP(A213,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":1.2685674263922118,"d":"1.27"}]
["01029","01","AL","029","Cleburne","","2104008610","Hydronic heater: outdoor","Hydronic heater",43.381607360496595,"A","CEC Survey",2017,15,"I",67.39829540432606,"TON",8,{"v":1.5536145271025419,"d":"1.55"},{"$f":"VLOOKUP(A214,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":1.268567426392212,"d":"1.27"}]
["01029","01","AL","029","Cleburne","","2104008620","Hydronic heater: indoor","Hydronic heater",27.716026924761717,"A","CEC Survey",2017,15,"I",43.06002206387499,"TON",8,{"v":1.5536145271025417,"d":"1.55"},{"$f":"VLOOKUP(A215,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":1.2685674263922118,"d":"1.27"}]
["01029","01","AL","029","Cleburne","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2050446489026834,"A","CEC Survey",2017,15,"I",1.8721748723423906,"TON",8,{"v":1.5536145271025414,"d":"1.55"},{"$f":"VLOOKUP(A216,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":1.2685674263922115,"d":"1.27"}]
["01029","01","AL","029","Cleburne","","2104008100","Fireplace: general","Fireplace: general",626.355051452,"A","CEC Survey",2017,15,"I",164.80123458903,"TON",8,{"v":0.26311152788979997,"d":"0.26"},{"$f":"VLOOKUP(A217,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.214837534,"d":"0.21"}]
["01029","01","AL","029","Cleburne","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",200.23802837924,"A","CEC Survey",2017,15,"I",121.68697689883493,"TON",8,{"v":0.6077116214327,"d":"0.61"},{"$f":"VLOOKUP(A218,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.496212641,"d":"0.50"}]
["01029","01","AL","029","Cleburne","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",264.83094075964,"A","CEC Survey",2017,15,"I",160.94084041458814,"TON",8,{"v":0.6077116214327,"d":"0.61"},{"$f":"VLOOKUP(A219,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.496212641,"d":"0.50"}]
["01029","01","AL","029","Cleburne","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",180.86015466512004,"A","CEC Survey",2017,15,"I",109.91081784410898,"TON",8,{"v":0.6077116214326999,"d":"0.61"},{"$f":"VLOOKUP(A220,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.4962126409999999,"d":"0.50"}]
["01029","01","AL","029","Cleburne","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,934.034550941,"A","CEC Survey",2017,15,"I",168.93708661239262,"TON",8,{"v":0.1808681343128,"d":"0.18"},{"$f":"VLOOKUP(A221,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.147683624,"d":"0.15"}]
["01029","01","AL","029","Cleburne","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",237.868890824,"A","CEC Survey",2017,15,"I",82.43834684977915,"TON",8,{"v":0.346570527,"d":"0.35"},{"$f":"VLOOKUP(A222,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.2829840181268883,"d":"0.28"}]
["01029","01","AL","029","Cleburne","","2104009000","Wax Log; Total: All Combustor Types",null,82.91743837582094,"A","CEC Survey",2017,15,"I",28.476232214610214,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A223,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.28041867396097003,"d":"0.28"}]
["01029","01","AL","029","Cleburne","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",290.87175302066004,"A","CEC Survey",2017,15,"I",287.54353924759,"TON",8,{"v":0.9885577965597998,"d":"0.99"},{"$f":"VLOOKUP(A224,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.8071836339999999,"d":"0.81"}]
["01029","01","AL","029","Cleburne","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",384.70135076926,"A","CEC Survey",2017,15,"I",380.2995196500384,"TON",8,{"v":0.9885577965598,"d":"0.99"},{"$f":"VLOOKUP(A225,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.807183634,"d":"0.81"}]
["01029","01","AL","029","Cleburne","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",262.72287369608006,"A","CEC Survey",2017,15,"I",259.7167451268555,"TON",8,{"v":0.9885577965597999,"d":"0.99"},{"$f":"VLOOKUP(A226,cordwood_density!A:D,4,FALSE)","v":1.2247},{"v":0.807183634,"d":"0.81"}]
["01031","01","AL","031","Coffee","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",70.32881501200474,"A","CEC Survey",2017,15,"I",104.07695261495505,"TON",8,{"v":1.4798621674087598,"d":"1.48"},{"$f":"VLOOKUP(A227,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":1.1877856709276504,"d":"1.19"}]
["01031","01","AL","031","Coffee","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.702336352324708,"A","CEC Survey",2017,15,"I",8.438671833645003,"TON",8,{"v":1.4798621674087598,"d":"1.48"},{"$f":"VLOOKUP(A228,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":1.1877856709276504,"d":"1.19"}]
["01031","01","AL","031","Coffee","","2104008610","Hydronic heater: outdoor","Hydronic heater",68.4280362278965,"A","CEC Survey",2017,15,"I",101.26406200374005,"TON",8,{"v":1.4798621674087598,"d":"1.48"},{"$f":"VLOOKUP(A229,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":1.1877856709276504,"d":"1.19"}]
["01031","01","AL","031","Coffee","","2104008620","Hydronic heater: indoor","Hydronic heater",43.71791203448943,"A","CEC Survey",2017,15,"I",64.69648405794503,"TON",8,{"v":1.4798621674087598,"d":"1.48"},{"$f":"VLOOKUP(A230,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":1.1877856709276504,"d":"1.19"}]
["01031","01","AL","031","Coffee","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.9007787841082362,"A","CEC Survey",2017,15,"I",2.8128906112150016,"TON",8,{"v":1.4798621674087598,"d":"1.48"},{"$f":"VLOOKUP(A231,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":1.1877856709276504,"d":"1.19"}]
["01031","01","AL","031","Coffee","","2104008100","Fireplace: general","Fireplace: general",1799.32016178,"A","CEC Survey",2017,15,"I",456.1415376232813,"TON",8,{"v":0.2535077121417,"d":"0.25"},{"$f":"VLOOKUP(A232,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.203473563,"d":"0.20"}]
["01031","01","AL","031","Coffee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",552.0704920128,"A","CEC Survey",2017,15,"I",279.1863030095729,"TON",8,{"v":0.5057077077090001,"d":"0.51"},{"$f":"VLOOKUP(A233,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.4058975100000001,"d":"0.41"}]
["01031","01","AL","031","Coffee","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",730.1577475007999,"A","CEC Survey",2017,15,"I",369.2464007545964,"TON",8,{"v":0.5057077077090001,"d":"0.51"},{"$f":"VLOOKUP(A234,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.4058975100000001,"d":"0.41"}]
["01031","01","AL","031","Coffee","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",498.6443153664,"A","CEC Survey",2017,15,"I",252.16827368606585,"TON",8,{"v":0.505707707709,"d":"0.51"},{"$f":"VLOOKUP(A235,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.40589750999999996,"d":"0.41"}]
["01031","01","AL","031","Coffee","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2913.45922548,"A","CEC Survey",2017,15,"I",531.5220055613347,"TON",8,{"v":0.1824367408038,"d":"0.18"},{"$f":"VLOOKUP(A236,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.146429682,"d":"0.15"}]
["01031","01","AL","031","Coffee","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",642.64864626,"A","CEC Survey",2017,15,"I",120.89185716033501,"TON",8,{"v":0.188115011,"d":"0.19"},{"$f":"VLOOKUP(A237,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.1509872469700618,"d":"0.15"}]
["01031","01","AL","031","Coffee","","2104009000","Wax Log; Total: All Combustor Types",null,281.8015141059426,"A","CEC Survey",2017,15,"I",65.97883664110678,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A238,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.18792222489766433,"d":"0.19"}]
["01031","01","AL","031","Coffee","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",651.2187150378,"A","CEC Survey",2017,15,"I",528.9459049340157,"TON",8,{"v":0.8122400243108999,"d":"0.81"},{"$f":"VLOOKUP(A239,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.651930351,"d":"0.65"}]
["01031","01","AL","031","Coffee","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",861.2892682757999,"A","CEC Survey",2017,15,"I",699.573616203053,"TON",8,{"v":0.8122400243109,"d":"0.81"},{"$f":"VLOOKUP(A240,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.6519303510000001,"d":"0.65"}]
["01031","01","AL","031","Coffee","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",588.1975490664,"A","CEC Survey",2017,15,"I",477.75759155330456,"TON",8,{"v":0.8122400243109,"d":"0.81"},{"$f":"VLOOKUP(A241,cordwood_density!A:D,4,FALSE)","v":1.2459},{"v":0.6519303510000001,"d":"0.65"}]
["01033","01","AL","033","Colbert","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",101.40465555748732,"A","CEC Survey",2017,15,"I",163.5127574263377,"TON",8,{"v":1.6124778150214285,"d":"1.61"},{"$f":"VLOOKUP(A242,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":1.2087539842739343,"d":"1.21"}]
["01033","01","AL","033","Colbert","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.221999099255727,"A","CEC Survey",2017,15,"I",13.25779114267603,"TON",8,{"v":1.6124778150214287,"d":"1.61"},{"$f":"VLOOKUP(A243,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":1.2087539842739345,"d":"1.21"}]
["01033","01","AL","033","Colbert","","2104008610","Hydronic heater: outdoor","Hydronic heater",98.66398919106874,"A","CEC Survey",2017,15,"I",159.09349371211238,"TON",8,{"v":1.6124778150214287,"d":"1.61"},{"$f":"VLOOKUP(A244,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":1.2087539842739345,"d":"1.21"}]
["01033","01","AL","033","Colbert","","2104008620","Hydronic heater: indoor","Hydronic heater",63.035326427627254,"A","CEC Survey",2017,15,"I",101.6430654271829,"TON",8,{"v":1.6124778150214285,"d":"1.61"},{"$f":"VLOOKUP(A245,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":1.2087539842739343,"d":"1.21"}]
["01033","01","AL","033","Colbert","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.740666366418576,"A","CEC Survey",2017,15,"I",4.419263714225344,"TON",8,{"v":1.6124778150214287,"d":"1.61"},{"$f":"VLOOKUP(A246,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":1.2087539842739345,"d":"1.21"}]
["01033","01","AL","033","Colbert","","2104008100","Fireplace: general","Fireplace: general",2403.7004687149997,"A","CEC Survey",2017,15,"I",623.7656549831493,"TON",8,{"v":0.25950223961,"d":"0.26"},{"$f":"VLOOKUP(A247,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.194529415,"d":"0.19"}]
["01033","01","AL","033","Colbert","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",520.95153737471,"A","CEC Survey",2017,15,"I",257.68590792867053,"TON",8,{"v":0.49464468274199985,"d":"0.49"},{"$f":"VLOOKUP(A248,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.3707981129999999,"d":"0.37"}]
["01033","01","AL","033","Colbert","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",689.00042039881,"A","CEC Survey",2017,15,"I",340.81039435727394,"TON",8,{"v":0.4946446827419999,"d":"0.49"},{"$f":"VLOOKUP(A249,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.37079811299999993,"d":"0.37"}]
["01033","01","AL","033","Colbert","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",470.53687246748,"A","CEC Survey",2017,15,"I",232.74856200008955,"TON",8,{"v":0.49464468274199996,"d":"0.49"},{"$f":"VLOOKUP(A250,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.37079811299999993,"d":"0.37"}]
["01033","01","AL","033","Colbert","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3367.065412672,"A","CEC Survey",2017,15,"I",661.1790688193944,"TON",8,{"v":0.196366564882,"d":"0.20"},{"$f":"VLOOKUP(A251,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.147201323,"d":"0.15"}]
["01033","01","AL","033","Colbert","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",762.9547041740001,"A","CEC Survey",2017,15,"I",161.79654248281986,"TON",8,{"v":0.212065725,"d":"0.21"},{"$f":"VLOOKUP(A252,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.1589698088455772,"d":"0.16"}]
["01033","01","AL","033","Colbert","","2104009000","Wax Log; Total: All Combustor Types",null,315.74121735937496,"A","CEC Survey",2017,15,"I",108.43461160120845,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A253,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.25744284107946025,"d":"0.26"}]
["01033","01","AL","033","Colbert","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",719.7034921906701,"A","CEC Survey",2017,15,"I",637.2216125137479,"TON",8,{"v":0.8853946374139999,"d":"0.89"},{"$f":"VLOOKUP(A254,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.6637141209999999,"d":"0.66"}]
["01033","01","AL","033","Colbert","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",951.86590902637,"A","CEC Survey",2017,15,"I",842.7769713891504,"TON",8,{"v":0.885394637414,"d":"0.89"},{"$f":"VLOOKUP(A255,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.663714121,"d":"0.66"}]
["01033","01","AL","033","Colbert","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",650.0547671399601,"A","CEC Survey",2017,15,"I",575.5550048511271,"TON",8,{"v":0.885394637414,"d":"0.89"},{"$f":"VLOOKUP(A256,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":0.663714121,"d":"0.66"}]
["01035","01","AL","035","Conecuh","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",23.270069507255275,"A","CEC Survey",2017,15,"I",35.686440265077714,"TON",8,{"v":1.5335768659372158,"d":"1.53"},{"$f":"VLOOKUP(A257,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":1.1984814519671896,"d":"1.20"}]
["01035","01","AL","035","Conecuh","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.8867623924801575,"A","CEC Survey",2017,15,"I",2.893495156627923,"TON",8,{"v":1.5335768659372155,"d":"1.53"},{"$f":"VLOOKUP(A258,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":1.1984814519671894,"d":"1.20"}]
["01035","01","AL","035","Conecuh","","2104008610","Hydronic heater: outdoor","Hydronic heater",22.64114870976189,"A","CEC Survey",2017,15,"I",34.72194187953507,"TON",8,{"$f":"P259/J259","v":{"v":1.5335768659372158,"d":"1.53"}},{"$f":"VLOOKUP(A259,cordwood_density!A:D,4,FALSE)","v":1.2796},{"$f":"S259/T259","v":{"v":1.1984814519671896,"d":"1.20"}}]
["01035","01","AL","035","Conecuh","","2104008620","Hydronic heater: indoor","Hydronic heater",14.465178342347874,"A","CEC Survey",2017,15,"I",22.183462867480742,"TON",8,{"v":1.5335768659372158,"d":"1.53"},{"$f":"VLOOKUP(A260,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":1.1984814519671896,"d":"1.20"}]
["01035","01","AL","035","Conecuh","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.6289207974933858,"A","CEC Survey",2017,15,"I",0.9644983855426409,"TON",8,{"v":1.5335768659372158,"d":"1.53"},{"$f":"VLOOKUP(A261,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":1.1984814519671896,"d":"1.20"}]
["01035","01","AL","035","Conecuh","","2104008100","Fireplace: general","Fireplace: general",491.57421714,"A","CEC Survey",2017,15,"I",135.85760383587098,"TON",8,{"v":0.2763725173104,"d":"0.28"},{"$f":"VLOOKUP(A262,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.215983524,"d":"0.22"}]
["01035","01","AL","035","Conecuh","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",144.80007965712,"A","CEC Survey",2017,15,"I",84.31971994470943,"TON",8,{"v":0.5823181875616,"d":"0.58"},{"$f":"VLOOKUP(A263,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.455078296,"d":"0.46"}]
["01035","01","AL","035","Conecuh","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",191.50978277232,"A","CEC Survey",2017,15,"I",111.51962960429312,"TON",8,{"v":0.5823181875616,"d":"0.58"},{"$f":"VLOOKUP(A264,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.455078296,"d":"0.46"}]
["01035","01","AL","035","Conecuh","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",130.78716872256,"A","CEC Survey",2017,15,"I",76.15974704683433,"TON",8,{"v":0.5823181875616,"d":"0.58"},{"$f":"VLOOKUP(A265,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.455078296,"d":"0.46"}]
["01035","01","AL","035","Conecuh","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,706.281440256,"A","CEC Survey",2017,15,"I",132.95544013642686,"TON",8,{"v":0.1882471102288,"d":"0.19"},{"$f":"VLOOKUP(A266,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.14711402799999998,"d":"0.15"}]
["01035","01","AL","035","Conecuh","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",169.032975336,"A","CEC Survey",2017,15,"I",40.31275846630435,"TON",8,{"v":0.23849049799999997,"d":"0.24"},{"$f":"VLOOKUP(A267,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.1863789449828071,"d":"0.19"}]
["01035","01","AL","035","Conecuh","","2104009000","Wax Log; Total: All Combustor Types",null,67.73577678509812,"A","CEC Survey",2017,15,"I",15.859133210981629,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A268,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.18297303844951546,"d":"0.18"}]
["01035","01","AL","035","Conecuh","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",183.61098031032,"A","CEC Survey",2017,15,"I",177.2923919843687,"TON",8,{"v":0.9655870889896002,"d":"0.97"},{"$f":"VLOOKUP(A269,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.7546007260000002,"d":"0.75"}]
["01035","01","AL","035","Conecuh","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",242.84032879752,"A","CEC Survey",2017,15,"I",234.4834861728747,"TON",8,{"v":0.9655870889896002,"d":"0.97"},{"$f":"VLOOKUP(A270,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.7546007260000002,"d":"0.75"}]
["01035","01","AL","035","Conecuh","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",165.84217576416003,"A","CEC Survey",2017,15,"I",160.1350637278169,"TON",8,{"v":0.9655870889896002,"d":"0.97"},{"$f":"VLOOKUP(A271,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.7546007260000002,"d":"0.75"}]
["01037","01","AL","037","Coosa","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",31.75318241807361,"A","CEC Survey",2017,15,"I",53.60631164323114,"TON",8,{"v":1.68821855199997,"d":"1.69"},{"$f":"VLOOKUP(A272,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":1.267145952112865,"d":"1.27"}]
["01037","01","AL","037","Coosa","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.5745823582221843,"A","CEC Survey",2017,15,"I",4.3464577008025245,"TON",8,{"v":1.6882185519999702,"d":"1.69"},{"$f":"VLOOKUP(A273,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":1.267145952112865,"d":"1.27"}]
["01037","01","AL","037","Coosa","","2104008610","Hydronic heater: outdoor","Hydronic heater",30.894988298666213,"A","CEC Survey",2017,15,"I",52.157492409630294,"TON",8,{"v":1.6882185519999702,"d":"1.69"},{"$f":"VLOOKUP(A274,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":1.267145952112865,"d":"1.27"}]
["01037","01","AL","037","Coosa","","2104008620","Hydronic heater: indoor","Hydronic heater",19.73846474637008,"A","CEC Survey",2017,15,"I",33.32284237281936,"TON",8,{"v":1.6882185519999704,"d":"1.69"},{"$f":"VLOOKUP(A275,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":1.2671459521128652,"d":"1.27"}]
["01037","01","AL","037","Coosa","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8581941194073949,"A","CEC Survey",2017,15,"I",1.4488192336008416,"TON",8,{"v":1.6882185519999702,"d":"1.69"},{"$f":"VLOOKUP(A276,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":1.267145952112865,"d":"1.27"}]
["01037","01","AL","037","Coosa","","2104008100","Fireplace: general","Fireplace: general",465.88419006,"A","CEC Survey",2017,15,"I",134.16461760899995,"TON",8,{"v":0.2879784729156,"d":"0.29"},{"$f":"VLOOKUP(A277,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.216151372,"d":"0.22"}]
["01037","01","AL","037","Coosa","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",143.60763991044,"A","CEC Survey",2017,15,"I",93.46675137851236,"TON",8,{"v":0.6508480428813,"d":"0.65"},{"$f":"VLOOKUP(A278,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.48851463100000003,"d":"0.49"}]
["01037","01","AL","037","Coosa","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",189.93268504284,"A","CEC Survey",2017,15,"I",123.61731633932278,"TON",8,{"v":0.6508480428813,"d":"0.65"},{"$f":"VLOOKUP(A279,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.48851463100000003,"d":"0.49"}]
["01037","01","AL","037","Coosa","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",129.71012637072002,"A","CEC Survey",2017,15,"I",84.42158189026922,"TON",8,{"v":0.6508480428812999,"d":"0.65"},{"$f":"VLOOKUP(A280,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.4885146309999999,"d":"0.49"}]
["01037","01","AL","037","Coosa","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,677.2741658919999,"A","CEC Survey",2017,15,"I",133.1784839669203,"TON",8,{"v":0.1966389546123,"d":"0.20"},{"$f":"VLOOKUP(A281,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.147593601,"d":"0.15"}]
["01037","01","AL","037","Coosa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",171.05533684000002,"A","CEC Survey",2017,15,"I",57.5414997626916,"TON",8,{"v":0.33639114,"d":"0.34"},{"$f":"VLOOKUP(A282,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.25248903400135103,"d":"0.25"}]
["01037","01","AL","037","Coosa","","2104009000","Wax Log; Total: All Combustor Types",null,60.38193503065151,"A","CEC Survey",2017,15,"I",20.736892470157862,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A283,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.25777133528484575,"d":"0.26"}]
["01037","01","AL","037","Coosa","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",207.85579238356001,"A","CEC Survey",2017,15,"I",224.8623324457832,"TON",8,{"v":1.0818189373854,"d":"1.08"},{"$f":"VLOOKUP(A284,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.8119934979999999,"d":"0.81"}]
["01037","01","AL","037","Coosa","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",274.90604799116,"A","CEC Survey",2017,15,"I",297.3985687186165,"TON",8,{"v":1.0818189373854001,"d":"1.08"},{"$f":"VLOOKUP(A285,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.8119934980000001,"d":"0.81"}]
["01037","01","AL","037","Coosa","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",187.74071570128,"A","CEC Survey",2017,15,"I",203.10146156393324,"TON",8,{"v":1.0818189373854001,"d":"1.08"},{"$f":"VLOOKUP(A286,cordwood_density!A:D,4,FALSE)","v":1.3323},{"v":0.8119934980000001,"d":"0.81"}]
["01039","01","AL","039","Covington","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",69.85037171536052,"A","CEC Survey",2017,15,"I",107.20092988224044,"TON",8,{"v":1.5347223965977308,"d":"1.53"},{"$f":"VLOOKUP(A287,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":1.1719016467606373,"d":"1.17"}]
["01039","01","AL","039","Covington","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.6635436525967995,"A","CEC Survey",2017,15,"I",8.691967287749225,"TON",8,{"v":1.5347223965977306,"d":"1.53"},{"$f":"VLOOKUP(A288,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":1.1719016467606371,"d":"1.17"}]
["01039","01","AL","039","Covington","","2104008610","Hydronic heater: outdoor","Hydronic heater",67.96252383116159,"A","CEC Survey",2017,15,"I",104.3036074529907,"TON",8,{"v":1.5347223965977308,"d":"1.53"},{"$f":"VLOOKUP(A289,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":1.1719016467606373,"d":"1.17"}]
["01039","01","AL","039","Covington","","2104008620","Hydronic heater: indoor","Hydronic heater",43.42050133657546,"A","CEC Survey",2017,15,"I",66.63841587274406,"TON",8,{"v":1.5347223965977306,"d":"1.53"},{"$f":"VLOOKUP(A290,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":1.1719016467606371,"d":"1.17"}]
["01039","01","AL","039","Covington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.8878478841989332,"A","CEC Survey",2017,15,"I",2.897322429249742,"TON",8,{"v":1.5347223965977306,"d":"1.53"},{"$f":"VLOOKUP(A291,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":1.1719016467606371,"d":"1.17"}]
["01039","01","AL","039","Covington","","2104008100","Fireplace: general","Fireplace: general",1698.736244235,"A","CEC Survey",2017,15,"I",466.89752827906784,"TON",8,{"v":0.27484992438559996,"d":"0.27"},{"$f":"VLOOKUP(A292,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.20987318599999996,"d":"0.21"}]
["01039","01","AL","039","Covington","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",447.89191776449996,"A","CEC Survey",2017,15,"I",252.8292626794643,"TON",8,{"v":0.5644872181248001,"d":"0.56"},{"$f":"VLOOKUP(A293,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.43103788800000004,"d":"0.43"}]
["01039","01","AL","039","Covington","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",592.3731815594999,"A","CEC Survey",2017,15,"I",334.38708935025926,"TON",8,{"v":0.5644872181248001,"d":"0.56"},{"$f":"VLOOKUP(A294,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.43103788800000004,"d":"0.43"}]
["01039","01","AL","039","Covington","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",404.547538626,"A","CEC Survey",2017,15,"I",228.36191467822584,"TON",8,{"v":0.5644872181248001,"d":"0.56"},{"$f":"VLOOKUP(A295,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.43103788800000004,"d":"0.43"}]
["01039","01","AL","039","Covington","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2417.18564355,"A","CEC Survey",2017,15,"I",467.2106987925959,"TON",8,{"v":0.19328705680480002,"d":"0.19"},{"$f":"VLOOKUP(A296,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.147592438,"d":"0.15"}]
["01039","01","AL","039","Covington","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",574.35071907,"A","CEC Survey",2017,15,"I",117.70304947541354,"TON",8,{"v":0.204932362,"d":"0.20"},{"$f":"VLOOKUP(A297,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.15648469914477703,"d":"0.16"}]
["01039","01","AL","039","Covington","","2104009000","Wax Log; Total: All Combustor Types",null,219.53802972014947,"A","CEC Survey",2017,15,"I",51.400943835846945,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A298,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.17878153634697613,"d":"0.18"}]
["01039","01","AL","039","Covington","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",560.1808622295,"A","CEC Survey",2017,15,"I",523.3016989857084,"TON",8,{"v":0.9341656137680001,"d":"0.93"},{"$f":"VLOOKUP(A299,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.7133213300000001,"d":"0.71"}]
["01039","01","AL","039","Covington","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",740.8843661745,"A","CEC Survey",2017,15,"I",692.1086986585175,"TON",8,{"v":0.9341656137680001,"d":"0.93"},{"$f":"VLOOKUP(A300,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.7133213300000001,"d":"0.71"}]
["01039","01","AL","039","Covington","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",505.9698110460001,"A","CEC Survey",2017,15,"I",472.6595990838657,"TON",8,{"v":0.9341656137680001,"d":"0.93"},{"$f":"VLOOKUP(A301,cordwood_density!A:D,4,FALSE)","v":1.3096},{"v":0.7133213300000001,"d":"0.71"}]
["01041","01","AL","041","Crenshaw","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",30.93092613325626,"A","CEC Survey",2017,15,"I",47.33269009211835,"TON",8,{"v":1.5302707034441903,"d":"1.53"},{"$f":"VLOOKUP(A302,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":1.17361047890497,"d":"1.17"}]
["01041","01","AL","041","Crenshaw","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.5079129297234806,"A","CEC Survey",2017,15,"I",3.8377856831447312,"TON",8,{"v":1.5302707034441905,"d":"1.53"},{"$f":"VLOOKUP(A303,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":1.17361047890497,"d":"1.17"}]
["01041","01","AL","041","Crenshaw","","2104008610","Hydronic heater: outdoor","Hydronic heater",30.094955156681767,"A","CEC Survey",2017,15,"I",46.05342819773677,"TON",8,{"v":1.5302707034441903,"d":"1.53"},{"$f":"VLOOKUP(A304,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":1.17361047890497,"d":"1.17"}]
["01041","01","AL","041","Crenshaw","","2104008620","Hydronic heater: indoor","Hydronic heater",19.22733246121335,"A","CEC Survey",2017,15,"I",29.423023570776273,"TON",8,{"v":1.5302707034441905,"d":"1.53"},{"$f":"VLOOKUP(A305,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":1.17361047890497,"d":"1.17"}]
["01041","01","AL","041","Crenshaw","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8359709765744936,"A","CEC Survey",2017,15,"I",1.279261894381577,"TON",8,{"v":1.5302707034441903,"d":"1.53"},{"$f":"VLOOKUP(A306,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":1.17361047890497,"d":"1.17"}]
["01041","01","AL","041","Crenshaw","","2104008100","Fireplace: general","Fireplace: general",554.998292664,"A","CEC Survey",2017,15,"I",160.91656594050625,"TON",8,{"v":0.28994065039030004,"d":"0.29"},{"$f":"VLOOKUP(A307,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.22236417700000002,"d":"0.22"}]
["01041","01","AL","041","Crenshaw","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",163.95719111466,"A","CEC Survey",2017,15,"I",96.92255976612483,"TON",8,{"v":0.5911455246775,"d":"0.59"},{"$f":"VLOOKUP(A308,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.453367225,"d":"0.45"}]
["01041","01","AL","041","Crenshaw","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",216.84660760326,"A","CEC Survey",2017,15,"I",128.1879016261651,"TON",8,{"v":0.5911455246774999,"d":"0.59"},{"$f":"VLOOKUP(A309,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.45336722499999993,"d":"0.45"}]
["01041","01","AL","041","Crenshaw","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",148.09036616808,"A","CEC Survey",2017,15,"I",87.54295720811277,"TON",8,{"v":0.5911455246775001,"d":"0.59"},{"$f":"VLOOKUP(A310,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.4533672250000001,"d":"0.45"}]
["01041","01","AL","041","Crenshaw","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,839.698424898,"A","CEC Survey",2017,15,"I",159.78552047620457,"TON",8,{"v":0.19028917494470002,"d":"0.19"},{"$f":"VLOOKUP(A311,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.145938473,"d":"0.15"}]
["01041","01","AL","041","Crenshaw","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",211.710766518,"A","CEC Survey",2017,15,"I",52.435106094439476,"TON",8,{"v":0.247673309,"d":"0.25"},{"$f":"VLOOKUP(A312,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.1899480857427717,"d":"0.19"}]
["01041","01","AL","041","Crenshaw","","2104009000","Wax Log; Total: All Combustor Types",null,76.9568049225097,"A","CEC Survey",2017,15,"I",18.018073737158517,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A313,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.1795630799907968,"d":"0.18"}]
["01041","01","AL","041","Crenshaw","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",226.17535260653997,"A","CEC Survey",2017,15,"I",230.48168852912625,"TON",8,{"v":1.0190398108059002,"d":"1.02"},{"$f":"VLOOKUP(A314,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.7815321810000001,"d":"0.78"}]
["01041","01","AL","041","Crenshaw","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",299.13514376994,"A","CEC Survey",2017,15,"I",304.8306203127153,"TON",8,{"v":1.0190398108059,"d":"1.02"},{"$f":"VLOOKUP(A315,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.781532181,"d":"0.78"}]
["01041","01","AL","041","Crenshaw","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",204.28741525752,"A","CEC Survey",2017,15,"I",208.17700899404954,"TON",8,{"v":1.0190398108059002,"d":"1.02"},{"$f":"VLOOKUP(A316,cordwood_density!A:D,4,FALSE)","v":1.3039},{"v":0.7815321810000001,"d":"0.78"}]
["01043","01","AL","043","Cullman","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",174.44880159369754,"A","CEC Survey",2017,15,"I",286.9249682442283,"TON",8,{"v":1.644751730152294,"d":"1.64"},{"$f":"VLOOKUP(A317,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":1.2663625886605283,"d":"1.27"}]
["01043","01","AL","043","Cullman","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.144497426516017,"A","CEC Survey",2017,15,"I",23.26418661439689,"TON",8,{"v":1.6447517301522943,"d":"1.64"},{"$f":"VLOOKUP(A318,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":1.2663625886605285,"d":"1.27"}]
["01043","01","AL","043","Cullman","","2104008610","Hydronic heater: outdoor","Hydronic heater",169.7339691181922,"A","CEC Survey",2017,15,"I",279.1702393727627,"TON",8,{"v":1.6447517301522943,"d":"1.64"},{"$f":"VLOOKUP(A319,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":1.2663625886605285,"d":"1.27"}]
["01043","01","AL","043","Cullman","","2104008620","Hydronic heater: indoor","Hydronic heater",108.4411469366228,"A","CEC Survey",2017,15,"I",178.3587640437095,"TON",8,{"v":1.644751730152294,"d":"1.64"},{"$f":"VLOOKUP(A320,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":1.2663625886605283,"d":"1.27"}]
["01043","01","AL","043","Cullman","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.7148324755053395,"A","CEC Survey",2017,15,"I",7.75472887146563,"TON",8,{"v":1.644751730152294,"d":"1.64"},{"$f":"VLOOKUP(A321,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":1.2663625886605283,"d":"1.27"}]
["01043","01","AL","043","Cullman","","2104008100","Fireplace: general","Fireplace: general",2398.6453900653432,"A","CEC Survey",2017,15,"I",641.2384112135678,"TON",8,{"v":0.2673335599624,"d":"0.27"},{"$f":"VLOOKUP(A322,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.205831198,"d":"0.21"}]
["01043","01","AL","043","Cullman","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",839.3828938096641,"A","CEC Survey",2017,15,"I",379.74474513949053,"TON",8,{"$f":"P323/J323","v":{"v":0.4524094402448,"d":"0.45"}},{"$f":"VLOOKUP(A323,cordwood_density!A:D,4,FALSE)","v":1.2988},{"$f":"S323/T323","v":{"v":0.348328796,"d":"0.35"}}]
["01043","01","AL","043","Cullman","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1110.1515692321364,"A","CEC Survey",2017,15,"I",502.2430500231971,"TON",8,{"v":0.45240944024479995,"d":"0.45"},{"$f":"VLOOKUP(A324,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.348328796,"d":"0.35"}]
["01043","01","AL","043","Cullman","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",758.1522911829225,"A","CEC Survey",2017,15,"I",342.9952536743786,"TON",8,{"v":0.45240944024480007,"d":"0.45"},{"$f":"VLOOKUP(A325,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.34832879600000005,"d":"0.35"}]
["01043","01","AL","043","Cullman","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4557.468445972565,"A","CEC Survey",2017,15,"I",874.378581047666,"TON",8,{"v":0.19185620074239995,"d":"0.19"},{"$f":"VLOOKUP(A326,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.14771804799999996,"d":"0.15"}]
["01043","01","AL","043","Cullman","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1127.5652169205962,"A","CEC Survey",2017,15,"I",293.88337300096896,"TON",8,{"v":0.260635366,"d":"0.26"},{"$f":"VLOOKUP(A327,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.20067398059747457,"d":"0.20"}]
["01043","01","AL","043","Cullman","","2104009000","Wax Log; Total: All Combustor Types",null,446.64534592102507,"A","CEC Survey",2017,15,"I",153.39085284297525,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A328,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.2644200415768402,"d":"0.26"}]
["01043","01","AL","043","Cullman","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1275.0571429764857,"A","CEC Survey",2017,15,"I",1193.5299794315288,"TON",8,{"v":0.9360599922959999,"d":"0.94"},{"$f":"VLOOKUP(A329,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.72071142,"d":"0.72"}]
["01043","01","AL","043","Cullman","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1686.3658987753518,"A","CEC Survey",2017,15,"I",1578.5396502158928,"TON",8,{"v":0.936059992296,"d":"0.94"},{"$f":"VLOOKUP(A330,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.72071142,"d":"0.72"}]
["01043","01","AL","043","Cullman","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1151.6645162368259,"A","CEC Survey",2017,15,"I",1078.0270781962197,"TON",8,{"v":0.9360599922959999,"d":"0.94"},{"$f":"VLOOKUP(A331,cordwood_density!A:D,4,FALSE)","v":1.2988},{"v":0.72071142,"d":"0.72"}]
["01045","01","AL","045","Dale","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",67.38274817350009,"A","CEC Survey",2017,15,"I",102.51698765181816,"TON",8,{"v":1.5214129792963158,"d":"1.52"},{"$f":"VLOOKUP(A332,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":1.18563979059875,"d":"1.19"}]
["01045","01","AL","045","Dale","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.463466068121629,"A","CEC Survey",2017,15,"I",8.312188187985255,"TON",8,{"v":1.5214129792963158,"d":"1.52"},{"$f":"VLOOKUP(A333,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":1.18563979059875,"d":"1.19"}]
["01045","01","AL","045","Dale","","2104008610","Hydronic heater: outdoor","Hydronic heater",65.56159281745954,"A","CEC Survey",2017,15,"I",99.74625825582307,"TON",8,{"v":1.5214129792963158,"d":"1.52"},{"$f":"VLOOKUP(A334,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":1.18563979059875,"d":"1.19"}]
["01045","01","AL","045","Dale","","2104008620","Hydronic heater: indoor","Hydronic heater",41.88657318893249,"A","CEC Survey",2017,15,"I",63.72677610788696,"TON",8,{"v":1.5214129792963158,"d":"1.52"},{"$f":"VLOOKUP(A335,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":1.18563979059875,"d":"1.19"}]
["01045","01","AL","045","Dale","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.821155356040543,"A","CEC Survey",2017,15,"I",2.7707293959950854,"TON",8,{"v":1.521412979296316,"d":"1.52"},{"$f":"VLOOKUP(A336,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":1.1856397905987501,"d":"1.19"}]
["01045","01","AL","045","Dale","","2104008100","Fireplace: general","Fireplace: general",1687.506828525,"A","CEC Survey",2017,15,"I",440.94242230958974,"TON",8,{"v":0.26129815586879995,"d":"0.26"},{"$f":"VLOOKUP(A337,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.20363010899999998,"d":"0.20"}]
["01045","01","AL","045","Dale","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",524.4909841394999,"A","CEC Survey",2017,15,"I",275.63506957137037,"TON",8,{"v":0.5255287086079999,"d":"0.53"},{"$f":"VLOOKUP(A338,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.40954544,"d":"0.41"}]
["01045","01","AL","045","Dale","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",693.6816241844999,"A","CEC Survey",2017,15,"I",364.54960814278013,"TON",8,{"v":0.5255287086079998,"d":"0.53"},{"$f":"VLOOKUP(A339,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.40954543999999987,"d":"0.41"}]
["01045","01","AL","045","Dale","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",473.733792126,"A","CEC Survey",2017,15,"I",248.96070799994746,"TON",8,{"v":0.5255287086079999,"d":"0.53"},{"$f":"VLOOKUP(A340,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.40954544,"d":"0.41"}]
["01045","01","AL","045","Dale","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2658.724873125,"A","CEC Survey",2017,15,"I",498.935062429625,"TON",8,{"v":0.18765953087999998,"d":"0.19"},{"$f":"VLOOKUP(A341,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.1462434,"d":"0.15"}]
["01045","01","AL","045","Dale","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",585.949604325,"A","CEC Survey",2017,15,"I",117.04045098043274,"TON",8,{"v":0.19974491,"d":"0.20"},{"$f":"VLOOKUP(A342,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.1556615570448878,"d":"0.16"}]
["01045","01","AL","045","Dale","","2104009000","Wax Log; Total: All Combustor Types",null,270.382951225503,"A","CEC Survey",2017,15,"I",63.30538225121484,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A343,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.18245971009975062,"d":"0.18"}]
["01045","01","AL","045","Dale","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",614.63090652375,"A","CEC Survey",2017,15,"I",528.9677958905069,"TON",8,{"v":0.8606267440767998,"d":"0.86"},{"$f":"VLOOKUP(A344,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.6706879239999999,"d":"0.67"}]
["01045","01","AL","045","Dale","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",812.89894088625,"A","CEC Survey",2017,15,"I",699.6025687584123,"TON",8,{"v":0.8606267440767998,"d":"0.86"},{"$f":"VLOOKUP(A345,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.6706879239999999,"d":"0.67"}]
["01045","01","AL","045","Dale","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",555.1504962150001,"A","CEC Survey",2017,15,"I",477.7773640301353,"TON",8,{"v":0.8606267440767997,"d":"0.86"},{"$f":"VLOOKUP(A346,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.6706879239999999,"d":"0.67"}]
["01047","01","AL","047","Dallas","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",53.92122269907479,"A","CEC Survey",2017,15,"I",79.5031335488587,"TON",8,{"v":1.4744312085160276,"d":"1.47"},{"$f":"VLOOKUP(A347,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.1081782852431623,"d":"1.11"}]
["01047","01","AL","047","Dallas","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.371991029654713,"A","CEC Survey",2017,15,"I",6.44620001747503,"TON",8,{"v":1.4744312085160274,"d":"1.47"},{"$f":"VLOOKUP(A348,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.1081782852431623,"d":"1.11"}]
["01047","01","AL","047","Dallas","","2104008610","Hydronic heater: outdoor","Hydronic heater",52.46389235585655,"A","CEC Survey",2017,15,"I",77.35440020970036,"TON",8,{"v":1.4744312085160276,"d":"1.47"},{"$f":"VLOOKUP(A349,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.1081782852431623,"d":"1.11"}]
["01047","01","AL","047","Dallas","","2104008620","Hydronic heater: indoor","Hydronic heater",33.518597894019464,"A","CEC Survey",2017,15,"I",49.4208668006419,"TON",8,{"v":1.4744312085160278,"d":"1.47"},{"$f":"VLOOKUP(A350,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.1081782852431625,"d":"1.11"}]
["01047","01","AL","047","Dallas","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.4573303432182376,"A","CEC Survey",2017,15,"I",2.1487333391583436,"TON",8,{"v":1.4744312085160278,"d":"1.47"},{"$f":"VLOOKUP(A351,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.1081782852431625,"d":"1.11"}]
["01047","01","AL","047","Dallas","","2104008100","Fireplace: general","Fireplace: general",2009.3610057859999,"A","CEC Survey",2017,15,"I",533.3822192821375,"TON",8,{"v":0.2654486763435,"d":"0.27"},{"$f":"VLOOKUP(A352,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.199510467,"d":"0.20"}]
["01047","01","AL","047","Dallas","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",343.2611783005,"A","CEC Survey",2017,15,"I",187.57810329257705,"TON",8,{"v":0.5464588341195,"d":"0.55"},{"$f":"VLOOKUP(A353,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.410716899,"d":"0.41"}]
["01047","01","AL","047","Dallas","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",453.99059065549994,"A","CEC Survey",2017,15,"I",248.0871688708277,"TON",8,{"v":0.5464588341195,"d":"0.55"},{"$f":"VLOOKUP(A354,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.410716899,"d":"0.41"}]
["01047","01","AL","047","Dallas","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",310.042354594,"A","CEC Survey",2017,15,"I",169.42538361910186,"TON",8,{"v":0.5464588341195,"d":"0.55"},{"$f":"VLOOKUP(A355,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.410716899,"d":"0.41"}]
["01047","01","AL","047","Dallas","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2188.380000803,"A","CEC Survey",2017,15,"I",420.14779359790157,"TON",8,{"v":0.191990327751,"d":"0.19"},{"$f":"VLOOKUP(A356,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.144299382,"d":"0.14"}]
["01047","01","AL","047","Dallas","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",465.906512201,"A","CEC Survey",2017,15,"I",80.34240194436877,"TON",8,{"v":0.172443183,"d":"0.17"},{"$f":"VLOOKUP(A357,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.12960780383314544,"d":"0.13"}]
["01047","01","AL","047","Dallas","","2104009000","Wax Log; Total: All Combustor Types",null,236.80232227648705,"A","CEC Survey",2017,15,"I",55.443072359935144,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A358,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.17597316798196166,"d":"0.18"}]
["01047","01","AL","047","Dallas","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",407.75617140648,"A","CEC Survey",2017,15,"I",372.5846521783828,"TON",8,{"v":0.9137437476255,"d":"0.91"},{"$f":"VLOOKUP(A359,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.686767191,"d":"0.69"}]
["01047","01","AL","047","Dallas","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",539.2904202472799,"A","CEC Survey",2017,15,"I",492.7732496552804,"TON",8,{"v":0.9137437476254999,"d":"0.91"},{"$f":"VLOOKUP(A360,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.6867671909999999,"d":"0.69"}]
["01047","01","AL","047","Dallas","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",368.29589675424006,"A","CEC Survey",2017,15,"I",336.5280729353135,"TON",8,{"v":0.9137437476254999,"d":"0.91"},{"$f":"VLOOKUP(A361,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.6867671909999999,"d":"0.69"}]
["01049","01","AL","049","De Kalb","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",166.3477798406465,"A","CEC Survey",2017,15,"I",272.8723075834221,"TON",8,{"v":1.6403724043977095,"d":"1.64"},{"$f":"VLOOKUP(A362,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":1.271606515036984,"d":"1.27"}]
["01049","01","AL","049","De Kalb","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.487657824917283,"A","CEC Survey",2017,15,"I",22.124781695953143,"TON",8,{"v":1.6403724043977093,"d":"1.64"},{"$f":"VLOOKUP(A363,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":1.271606515036984,"d":"1.27"}]
["01049","01","AL","049","De Kalb","","2104008610","Hydronic heater: outdoor","Hydronic heater",161.8518938990074,"A","CEC Survey",2017,15,"I",265.49738035143776,"TON",8,{"v":1.6403724043977097,"d":"1.64"},{"$f":"VLOOKUP(A364,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":1.2716065150369842,"d":"1.27"}]
["01049","01","AL","049","De Kalb","","2104008620","Hydronic heater: indoor","Hydronic heater",103.40537665769918,"A","CEC Survey",2017,15,"I",169.6233263356408,"TON",8,{"v":1.6403724043977095,"d":"1.64"},{"$f":"VLOOKUP(A365,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":1.271606515036984,"d":"1.27"}]
["01049","01","AL","049","De Kalb","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.495885941639095,"A","CEC Survey",2017,15,"I",7.3749272319843815,"TON",8,{"v":1.6403724043977093,"d":"1.64"},{"$f":"VLOOKUP(A366,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":1.271606515036984,"d":"1.27"}]
["01049","01","AL","049","De Kalb","","2104008100","Fireplace: general","Fireplace: general",1874.6972862396947,"A","CEC Survey",2017,15,"I",531.4015522301953,"TON",8,{"v":0.28345992504,"d":"0.28"},{"$f":"VLOOKUP(A367,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.219736376,"d":"0.22"}]
["01049","01","AL","049","De Kalb","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",707.2447575664669,"A","CEC Survey",2017,15,"I",313.8535244033013,"TON",8,{"v":0.44376931896,"d":"0.44"},{"$f":"VLOOKUP(A368,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.344007224,"d":"0.34"}]
["01049","01","AL","049","De Kalb","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",935.388227749198,"A","CEC Survey",2017,15,"I",415.096596791463,"TON",8,{"v":0.44376931896000005,"d":"0.44"},{"$f":"VLOOKUP(A369,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.344007224,"d":"0.34"}]
["01049","01","AL","049","De Kalb","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",638.8017165116476,"A","CEC Survey",2017,15,"I",283.4806026868528,"TON",8,{"v":0.44376931896,"d":"0.44"},{"$f":"VLOOKUP(A370,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.344007224,"d":"0.34"}]
["01049","01","AL","049","De Kalb","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3874.4192025084535,"A","CEC Survey",2017,15,"I",738.0150747682802,"TON",8,{"v":0.19048405353,"d":"0.19"},{"$f":"VLOOKUP(A371,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.14766205699999999,"d":"0.15"}]
["01049","01","AL","049","De Kalb","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1018.469392497682,"A","CEC Survey",2017,15,"I",277.791565034884,"TON",8,{"v":0.272753965,"d":"0.27"},{"$f":"VLOOKUP(A372,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.2114371821705426,"d":"0.21"}]
["01049","01","AL","049","De Kalb","","2104009000","Wax Log; Total: All Combustor Types",null,365.9972571491154,"A","CEC Survey",2017,15,"I",125.69398052614926,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A373,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.2662238372093023,"d":"0.27"}]
["01049","01","AL","049","De Kalb","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1161.6956571454887,"A","CEC Survey",2017,15,"I",1124.0385618984208,"TON",8,{"v":0.9675843711600002,"d":"0.97"},{"$f":"VLOOKUP(A374,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.7500654040000001,"d":"0.75"}]
["01049","01","AL","049","De Kalb","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1536.4361917085496,"A","CEC Survey",2017,15,"I",1486.631646381782,"TON",8,{"v":0.96758437116,"d":"0.97"},{"$f":"VLOOKUP(A375,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.750065404,"d":"0.75"}]
["01049","01","AL","049","De Kalb","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1049.2734967765705,"A","CEC Survey",2017,15,"I",1015.2606365534123,"TON",8,{"v":0.9675843711600001,"d":"0.97"},{"$f":"VLOOKUP(A376,cordwood_density!A:D,4,FALSE)","v":1.29},{"v":0.750065404,"d":"0.75"}]
["01051","01","AL","051","Elmore","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",142.99245408124298,"A","CEC Survey",2017,15,"I",224.20785467814238,"TON",8,{"v":1.5679698353226097,"d":"1.57"},{"$f":"VLOOKUP(A377,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":1.2213505494022507,"d":"1.22"}]
["01051","01","AL","051","Elmore","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.593982763344027,"A","CEC Survey",2017,15,"I",18.17901524417371,"TON",8,{"v":1.5679698353226097,"d":"1.57"},{"$f":"VLOOKUP(A378,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":1.2213505494022507,"d":"1.22"}]
["01051","01","AL","051","Elmore","","2104008610","Hydronic heater: outdoor","Hydronic heater",139.1277931601283,"A","CEC Survey",2017,15,"I",218.1481829300845,"TON",8,{"v":1.5679698353226097,"d":"1.57"},{"$f":"VLOOKUP(A379,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":1.2213505494022507,"d":"1.22"}]
["01051","01","AL","051","Elmore","","2104008620","Hydronic heater: indoor","Hydronic heater",88.88720118563754,"A","CEC Survey",2017,15,"I",139.37245020533177,"TON",8,{"v":1.5679698353226097,"d":"1.57"},{"$f":"VLOOKUP(A380,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":1.2213505494022507,"d":"1.22"}]
["01051","01","AL","051","Elmore","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.864660921114676,"A","CEC Survey",2017,15,"I",6.0596717480579025,"TON",8,{"v":1.5679698353226095,"d":"1.57"},{"$f":"VLOOKUP(A381,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":1.2213505494022507,"d":"1.22"}]
["01051","01","AL","051","Elmore","","2104008100","Fireplace: general","Fireplace: general",3096.684530865,"A","CEC Survey",2017,15,"I",782.4214879357982,"TON",8,{"v":0.25266425434600004,"d":"0.25"},{"$f":"VLOOKUP(A382,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.19680967000000002,"d":"0.20"}]
["01051","01","AL","051","Elmore","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",812.1263804343,"A","CEC Survey",2017,15,"I",428.2744838642862,"TON",8,{"v":0.5273495532004,"d":"0.53"},{"$f":"VLOOKUP(A383,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.410772358,"d":"0.41"}]
["01051","01","AL","051","Elmore","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1074.1026321872998,"A","CEC Survey",2017,15,"I",566.4275431753463,"TON",8,{"v":0.5273495532004001,"d":"0.53"},{"$f":"VLOOKUP(A384,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.41077235800000006,"d":"0.41"}]
["01051","01","AL","051","Elmore","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",733.5335049084,"A","CEC Survey",2017,15,"I",386.82856607096824,"TON",8,{"v":0.5273495532004001,"d":"0.53"},{"$f":"VLOOKUP(A385,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.41077235800000006,"d":"0.41"}]
["01051","01","AL","051","Elmore","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4501.9744509150005,"A","CEC Survey",2017,15,"I",856.8295875928975,"TON",8,{"v":0.19032306756400003,"d":"0.19"},{"$f":"VLOOKUP(A386,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.14824978000000003,"d":"0.15"}]
["01051","01","AL","051","Elmore","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1049.89138371,"A","CEC Survey",2017,15,"I",251.2725773489057,"TON",8,{"$f":"P387/J387","v":{"v":0.239331974,"d":"0.24"}},{"$f":"VLOOKUP(A387,cordwood_density!A:D,4,FALSE)","v":1.2838},{"$f":"S387/T387","v":{"v":0.1864246564885496,"d":"0.19"}}]
["01051","01","AL","051","Elmore","","2104009000","Wax Log; Total: All Combustor Types",null,418.177934923268,"A","CEC Survey",2017,15,"I",97.90896171283507,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A388,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.18237443527029132,"d":"0.18"}]
["01051","01","AL","051","Elmore","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1073.8627571961001,"A","CEC Survey",2017,15,"I",950.7891112512616,"TON",8,{"v":0.8853916432802001,"d":"0.89"},{"$f":"VLOOKUP(A389,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.6896647790000001,"d":"0.69"}]
["01051","01","AL","051","Elmore","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1420.2700982271,"A","CEC Survey",2017,15,"I",1257.4952761710233,"TON",8,{"v":0.8853916432802,"d":"0.89"},{"$f":"VLOOKUP(A390,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.689664779,"d":"0.69"}]
["01051","01","AL","051","Elmore","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",969.9405548868002,"A","CEC Survey",2017,15,"I",858.7772617753332,"TON",8,{"v":0.8853916432802001,"d":"0.89"},{"$f":"VLOOKUP(A391,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.6896647790000001,"d":"0.69"}]
["01053","01","AL","053","Escambia","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",52.33014927594508,"A","CEC Survey",2017,15,"I",81.29247433092199,"TON",8,{"v":1.5534538971454874,"d":"1.55"},{"$f":"VLOOKUP(A392,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":1.1784660120964099,"d":"1.18"}]
["01053","01","AL","053","Escambia","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.2429850764279795,"A","CEC Survey",2017,15,"I",6.591281702507188,"TON",8,{"v":1.5534538971454872,"d":"1.55"},{"$f":"VLOOKUP(A393,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":1.1784660120964097,"d":"1.18"}]
["01053","01","AL","053","Escambia","","2104008610","Hydronic heater: outdoor","Hydronic heater",50.915820917135754,"A","CEC Survey",2017,15,"I",79.09538043008625,"TON",8,{"v":1.5534538971454872,"d":"1.55"},{"$f":"VLOOKUP(A394,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":1.1784660120964097,"d":"1.18"}]
["01053","01","AL","053","Escambia","","2104008620","Hydronic heater: indoor","Hydronic heater",32.529552252614515,"A","CEC Survey",2017,15,"I",50.53315971922178,"TON",8,{"v":1.5534538971454872,"d":"1.55"},{"$f":"VLOOKUP(A395,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":1.1784660120964097,"d":"1.18"}]
["01053","01","AL","053","Escambia","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.4143283588093265,"A","CEC Survey",2017,15,"I",2.1970939008357293,"TON",8,{"v":1.5534538971454872,"d":"1.55"},{"$f":"VLOOKUP(A396,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":1.1784660120964097,"d":"1.18"}]
["01053","01","AL","053","Escambia","","2104008100","Fireplace: general","Fireplace: general",1246.039262196,"A","CEC Survey",2017,15,"I",338.90955963385284,"TON",8,{"v":0.2719894708908,"d":"0.27"},{"$f":"VLOOKUP(A397,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.206333994,"d":"0.21"}]
["01053","01","AL","053","Escambia","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",376.53746442371994,"A","CEC Survey",2017,15,"I",206.70253592835667,"TON",8,{"v":0.5489560945674001,"d":"0.55"},{"$f":"VLOOKUP(A398,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.4164437070000001,"d":"0.42"}]
["01053","01","AL","053","Escambia","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",498.0011626249199,"A","CEC Survey",2017,15,"I",273.38077332460074,"TON",8,{"v":0.5489560945674001,"d":"0.55"},{"$f":"VLOOKUP(A399,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.4164437070000001,"d":"0.42"}]
["01053","01","AL","053","Escambia","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",340.09835496336,"A","CEC Survey",2017,15,"I",186.69906470948345,"TON",8,{"v":0.5489560945674,"d":"0.55"},{"$f":"VLOOKUP(A400,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.416443707,"d":"0.42"}]
["01053","01","AL","053","Escambia","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1927.031585856,"A","CEC Survey",2017,15,"I",373.49945921403344,"TON",8,{"v":0.19382114022180003,"d":"0.19"},{"$f":"VLOOKUP(A401,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.14703469900000002,"d":"0.15"}]
["01053","01","AL","053","Escambia","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",444.46250746000004,"A","CEC Survey",2017,15,"I",89.54620139178441,"TON",8,{"v":0.201470765,"d":"0.20"},{"$f":"VLOOKUP(A402,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.1528377825823092,"d":"0.15"}]
["01053","01","AL","053","Escambia","","2104009000","Wax Log; Total: All Combustor Types",null,189.96467000841983,"A","CEC Survey",2017,15,"I",44.47686510781235,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A403,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.17761515703231678,"d":"0.18"}]
["01053","01","AL","053","Escambia","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",454.44586562998,"A","CEC Survey",2017,15,"I",415.75486914775337,"TON",8,{"v":0.9148611541914,"d":"0.91"},{"$f":"VLOOKUP(A404,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.694023027,"d":"0.69"}]
["01053","01","AL","053","Escambia","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",601.0413061557799,"A","CEC Survey",2017,15,"I",549.8693430663834,"TON",8,{"v":0.9148611541914,"d":"0.91"},{"$f":"VLOOKUP(A405,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.694023027,"d":"0.69"}]
["01053","01","AL","053","Escambia","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",410.46723347224,"A","CEC Survey",2017,15,"I",375.52052697216436,"TON",8,{"v":0.9148611541914,"d":"0.91"},{"$f":"VLOOKUP(A406,cordwood_density!A:D,4,FALSE)","v":1.3182},{"v":0.694023027,"d":"0.69"}]
["01055","01","AL","055","Etowah","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",148.5730109335583,"A","CEC Survey",2017,15,"I",221.96498040777354,"TON",8,{"v":1.4939791487905973,"d":"1.49"},{"$f":"VLOOKUP(A407,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":1.1538300500390775,"d":"1.15"}]
["01055","01","AL","055","Etowah","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",12.046460345964187,"A","CEC Survey",2017,15,"I",17.99716057360326,"TON",8,{"v":1.4939791487905973,"d":"1.49"},{"$f":"VLOOKUP(A408,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":1.1538300500390775,"d":"1.15"}]
["01055","01","AL","055","Etowah","","2104008610","Hydronic heater: outdoor","Hydronic heater",144.55752415157022,"A","CEC Survey",2017,15,"I",215.96592688323912,"TON",8,{"v":1.4939791487905976,"d":"1.49"},{"$f":"VLOOKUP(A409,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":1.1538300500390775,"d":"1.15"}]
["01055","01","AL","055","Etowah","","2104008620","Hydronic heater: indoor","Hydronic heater",92.35619598572544,"A","CEC Survey",2017,15,"I",137.97823106429166,"TON",8,{"v":1.4939791487905973,"d":"1.49"},{"$f":"VLOOKUP(A410,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":1.1538300500390775,"d":"1.15"}]
["01055","01","AL","055","Etowah","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.015486781988062,"A","CEC Survey",2017,15,"I",5.99905352453442,"TON",8,{"v":1.4939791487905976,"d":"1.49"},{"$f":"VLOOKUP(A411,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":1.1538300500390775,"d":"1.15"}]
["01055","01","AL","055","Etowah","","2104008100","Fireplace: general","Fireplace: general",5344.760143954,"A","CEC Survey",2017,15,"I",1263.705237344444,"TON",8,{"v":0.2364381568692,"d":"0.24"},{"$f":"VLOOKUP(A412,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.182605929,"d":"0.18"}]
["01055","01","AL","055","Etowah","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",873.5693645857199,"A","CEC Survey",2017,15,"I",450.3891163822007,"TON",8,{"v":0.5155733873471999,"d":"0.52"},{"$f":"VLOOKUP(A413,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.39818766399999994,"d":"0.40"}]
["01055","01","AL","055","Etowah","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1155.3659338069199,"A","CEC Survey",2017,15,"I",595.6759281183944,"TON",8,{"v":0.5155733873471998,"d":"0.52"},{"$f":"VLOOKUP(A414,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.3981876639999999,"d":"0.40"}]
["01055","01","AL","055","Etowah","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",789.03039381936,"A","CEC Survey",2017,15,"I",406.8030728613426,"TON",8,{"v":0.5155733873471999,"d":"0.52"},{"$f":"VLOOKUP(A415,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.39818766399999994,"d":"0.40"}]
["01055","01","AL","055","Etowah","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5886.984634234001,"A","CEC Survey",2017,15,"I",1129.4976150724228,"TON",8,{"v":0.19186352356080003,"d":"0.19"},{"$f":"VLOOKUP(A416,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.14818004600000004,"d":"0.15"}]
["01055","01","AL","055","Etowah","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1273.025449883,"A","CEC Survey",2017,15,"I",244.3486460023315,"TON",8,{"v":0.191943253,"d":"0.19"},{"$f":"VLOOKUP(A417,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.14824162264442386,"d":"0.15"}]
["01055","01","AL","055","Etowah","","2104009000","Wax Log; Total: All Combustor Types",null,561.0320561922642,"A","CEC Survey",2017,15,"I",192.67453776803907,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A418,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.2652369091751622,"d":"0.27"}]
["01055","01","AL","055","Etowah","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1080.06820113214,"A","CEC Survey",2017,15,"I",895.0254103450123,"TON",8,{"v":0.8286749016468,"d":"0.83"},{"$f":"VLOOKUP(A419,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.640002241,"d":"0.64"}]
["01055","01","AL","055","Etowah","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1428.47729827154,"A","CEC Survey",2017,15,"I",1183.743284649855,"TON",8,{"v":0.8286749016468,"d":"0.83"},{"$f":"VLOOKUP(A420,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.640002241,"d":"0.64"}]
["01055","01","AL","055","Etowah","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",975.54547199032,"A","CEC Survey",2017,15,"I",808.4100480535596,"TON",8,{"v":0.8286749016468001,"d":"0.83"},{"$f":"VLOOKUP(A421,cordwood_density!A:D,4,FALSE)","v":1.2948},{"v":0.6400022410000001,"d":"0.64"}]
["01057","01","AL","057","Fayette","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",47.26298969628413,"A","CEC Survey",2017,15,"I",75.56549507986706,"TON",8,{"v":1.598830196004467,"d":"1.60"},{"$f":"VLOOKUP(A422,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":1.2293965367200823,"d":"1.23"}]
["01057","01","AL","057","Fayette","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.8321342996987133,"A","CEC Survey",2017,15,"I",6.126932033502735,"TON",8,{"v":1.598830196004467,"d":"1.60"},{"$f":"VLOOKUP(A423,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":1.2293965367200823,"d":"1.23"}]
["01057","01","AL","057","Fayette","","2104008610","Hydronic heater: outdoor","Hydronic heater",45.98561159638456,"A","CEC Survey",2017,15,"I",73.52318440203281,"TON",8,{"v":1.5988301960044669,"d":"1.60"},{"$f":"VLOOKUP(A424,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":1.229396536720082,"d":"1.23"}]
["01057","01","AL","057","Fayette","","2104008620","Hydronic heater: indoor","Hydronic heater",29.37969629769014,"A","CEC Survey",2017,15,"I",46.973145590187634,"TON",8,{"v":1.5988301960044669,"d":"1.60"},{"$f":"VLOOKUP(A425,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":1.229396536720082,"d":"1.23"}]
["01057","01","AL","057","Fayette","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2773780998995712,"A","CEC Survey",2017,15,"I",2.042310677834245,"TON",8,{"v":1.5988301960044669,"d":"1.60"},{"$f":"VLOOKUP(A426,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":1.229396536720082,"d":"1.23"}]
["01057","01","AL","057","Fayette","","2104008100","Fireplace: general","Fireplace: general",921.98872649,"A","CEC Survey",2017,15,"I",247.77701821175935,"TON",8,{"v":0.2687419174365,"d":"0.27"},{"$f":"VLOOKUP(A427,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.206645073,"d":"0.21"}]
["01057","01","AL","057","Fayette","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",213.74816230689999,"A","CEC Survey",2017,15,"I",141.23454279952898,"TON",8,{"v":0.6607520798084999,"d":"0.66"},{"$f":"VLOOKUP(A428,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.5080754169999999,"d":"0.51"}]
["01057","01","AL","057","Fayette","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",282.69918240589993,"A","CEC Survey",2017,15,"I",186.79407273486092,"TON",8,{"v":0.6607520798085001,"d":"0.66"},{"$f":"VLOOKUP(A429,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.5080754170000001,"d":"0.51"}]
["01057","01","AL","057","Fayette","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",193.0628562772,"A","CEC Survey",2017,15,"I",127.56668381892942,"TON",8,{"v":0.6607520798084999,"d":"0.66"},{"$f":"VLOOKUP(A430,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.5080754169999999,"d":"0.51"}]
["01057","01","AL","057","Fayette","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1119.793913225,"A","CEC Survey",2017,15,"I",214.28850145231488,"TON",8,{"v":0.19136423133000002,"d":"0.19"},{"$f":"VLOOKUP(A431,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.14714666,"d":"0.15"}]
["01057","01","AL","057","Fayette","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",270.240718865,"A","CEC Survey",2017,15,"I",82.78618336857069,"TON",8,{"v":0.306342374,"d":"0.31"},{"$f":"VLOOKUP(A432,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.23555738100730486,"d":"0.24"}]
["01057","01","AL","057","Fayette","","2104009000","Wax Log; Total: All Combustor Types",null,99.89447148862543,"A","CEC Survey",2017,15,"I",34.30663347524927,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A433,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.2640743944636678,"d":"0.26"}]
["01057","01","AL","057","Fayette","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",295.1821104375,"A","CEC Survey",2017,15,"I",297.67797628613994,"TON",8,{"v":1.0084553425169998,"d":"1.01"},{"$f":"VLOOKUP(A434,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.7754366339999998,"d":"0.78"}]
["01057","01","AL","057","Fayette","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",390.4021460625,"A","CEC Survey",2017,15,"I",393.70312992683023,"TON",8,{"v":1.008455342517,"d":"1.01"},{"$f":"VLOOKUP(A435,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.775436634,"d":"0.78"}]
["01057","01","AL","057","Fayette","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",266.61609975000005,"A","CEC Survey",2017,15,"I",268.87043019393286,"TON",8,{"v":1.0084553425169998,"d":"1.01"},{"$f":"VLOOKUP(A436,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.7754366339999998,"d":"0.78"}]
["01059","01","AL","059","Franklin","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",69.7007192463463,"A","CEC Survey",2017,15,"I",112.68226199409911,"TON",8,{"v":1.6166585253710406,"d":"1.62"},{"$f":"VLOOKUP(A437,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.2150759303803387,"d":"1.22"}]
["01059","01","AL","059","Franklin","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.651409668622672,"A","CEC Survey",2017,15,"I",9.136399621143172,"TON",8,{"v":1.6166585253710408,"d":"1.62"},{"$f":"VLOOKUP(A438,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.215075930380339,"d":"1.22"}]
["01059","01","AL","059","Franklin","","2104008610","Hydronic heater: outdoor","Hydronic heater",67.81691602347206,"A","CEC Survey",2017,15,"I",109.63679545371805,"TON",8,{"v":1.6166585253710408,"d":"1.62"},{"$f":"VLOOKUP(A439,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.215075930380339,"d":"1.22"}]
["01059","01","AL","059","Franklin","","2104008620","Hydronic heater: indoor","Hydronic heater",43.327474126107155,"A","CEC Survey",2017,15,"I",70.04573042876432,"TON",8,{"v":1.6166585253710408,"d":"1.62"},{"$f":"VLOOKUP(A440,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.215075930380339,"d":"1.22"}]
["01059","01","AL","059","Franklin","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.8838032228742243,"A","CEC Survey",2017,15,"I",3.045466540381057,"TON",8,{"v":1.6166585253710406,"d":"1.62"},{"$f":"VLOOKUP(A441,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":1.2150759303803387,"d":"1.22"}]
["01059","01","AL","059","Franklin","","2104008100","Fireplace: general","Fireplace: general",1487.638521491,"A","CEC Survey",2017,15,"I",401.4486561403627,"TON",8,{"v":0.2698563194895,"d":"0.27"},{"$f":"VLOOKUP(A442,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.20282323900000002,"d":"0.20"}]
["01059","01","AL","059","Franklin","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",272.43125321812,"A","CEC Survey",2017,15,"I",151.4129638829979,"TON",8,{"v":0.5557841183580001,"d":"0.56"},{"$f":"VLOOKUP(A443,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.4177257560000001,"d":"0.42"}]
["01059","01","AL","059","Franklin","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",360.31230264332,"A","CEC Survey",2017,15,"I",200.2558554581585,"TON",8,{"v":0.555784118358,"d":"0.56"},{"$f":"VLOOKUP(A444,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.417725756,"d":"0.42"}]
["01059","01","AL","059","Franklin","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",246.06693839056004,"A","CEC Survey",2017,15,"I",136.76009641044973,"TON",8,{"v":0.5557841183580001,"d":"0.56"},{"$f":"VLOOKUP(A445,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.4177257560000001,"d":"0.42"}]
["01059","01","AL","059","Franklin","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1761.110505248,"A","CEC Survey",2017,15,"I",345.3700364547979,"TON",8,{"v":0.196109236431,"d":"0.20"},{"$f":"VLOOKUP(A446,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.147395142,"d":"0.15"}]
["01059","01","AL","059","Franklin","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",429.080029018,"A","CEC Survey",2017,15,"I",110.01817773711441,"TON",8,{"v":0.256404797,"d":"0.26"},{"$f":"VLOOKUP(A447,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.19271311311537018,"d":"0.19"}]
["01059","01","AL","059","Franklin","","2104009000","Wax Log; Total: All Combustor Types",null,165.64815811334537,"A","CEC Survey",2017,15,"I",56.88833988066856,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A448,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.25812006764374296,"d":"0.26"}]
["01059","01","AL","059","Franklin","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",411.40461561152995,"A","CEC Survey",2017,15,"I",408.8019471833865,"TON",8,{"v":0.9936737014379999,"d":"0.99"},{"$f":"VLOOKUP(A449,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.746842316,"d":"0.75"}]
["01059","01","AL","059","Franklin","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",544.1157819378299,"A","CEC Survey",2017,15,"I",540.673543048995,"TON",8,{"v":0.9936737014379999,"d":"0.99"},{"$f":"VLOOKUP(A450,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.746842316,"d":"0.75"}]
["01059","01","AL","059","Franklin","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",371.59126571364,"A","CEC Survey",2017,15,"I",369.240468423704,"TON",8,{"$f":"P451/J451","v":{"v":0.9936737014379999,"d":"0.99"}},{"$f":"VLOOKUP(A451,cordwood_density!A:D,4,FALSE)","v":1.3305},{"$f":"S451/T451","v":{"v":0.746842316,"d":"0.75"}}]
["01061","01","AL","061","Geneva","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",48.595485598402874,"A","CEC Survey",2017,15,"I",72.08722140346788,"TON",8,{"v":1.4834139532878148,"d":"1.48"},{"$f":"VLOOKUP(A452,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":1.205733522951975,"d":"1.21"}]
["01061","01","AL","061","Geneva","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.9401745079786115,"A","CEC Survey",2017,15,"I",5.844909843524423,"TON",8,{"v":1.483413953287815,"d":"1.48"},{"$f":"VLOOKUP(A453,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":1.2057335229519752,"d":"1.21"}]
["01061","01","AL","061","Geneva","","2104008610","Hydronic heater: outdoor","Hydronic heater",47.28209409574334,"A","CEC Survey",2017,15,"I",70.13891812229308,"TON",8,{"v":1.4834139532878148,"d":"1.48"},{"$f":"VLOOKUP(A454,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":1.205733522951975,"d":"1.21"}]
["01061","01","AL","061","Geneva","","2104008620","Hydronic heater: indoor","Hydronic heater",30.208004561169357,"A","CEC Survey",2017,15,"I",44.81097546702058,"TON",8,{"v":1.483413953287815,"d":"1.48"},{"$f":"VLOOKUP(A455,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":1.2057335229519752,"d":"1.21"}]
["01061","01","AL","061","Geneva","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.3133915026595373,"A","CEC Survey",2017,15,"I",1.9483032811748078,"TON",8,{"v":1.4834139532878148,"d":"1.48"},{"$f":"VLOOKUP(A456,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":1.205733522951975,"d":"1.21"}]
["01061","01","AL","061","Geneva","","2104008100","Fireplace: general","Fireplace: general",687.8754718160001,"A","CEC Survey",2017,15,"I",193.77851215763954,"TON",8,{"v":0.2817058030083,"d":"0.28"},{"$f":"VLOOKUP(A457,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.228973261,"d":"0.23"}]
["01061","01","AL","061","Geneva","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",309.33328273619,"A","CEC Survey",2017,15,"I",125.18897584150626,"TON",8,{"v":0.404705807064,"d":"0.40"},{"$f":"VLOOKUP(A458,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.32894888,"d":"0.33"}]
["01061","01","AL","061","Geneva","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",409.11821265108995,"A","CEC Survey",2017,15,"I",165.57251643554054,"TON",8,{"v":0.404705807064,"d":"0.40"},{"$f":"VLOOKUP(A459,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.32894888,"d":"0.33"}]
["01061","01","AL","061","Geneva","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",279.39780376172,"A","CEC Survey",2017,15,"I",113.073913663296,"TON",8,{"v":0.404705807064,"d":"0.40"},{"$f":"VLOOKUP(A460,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.32894888,"d":"0.33"}]
["01061","01","AL","061","Geneva","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1594.149630254,"A","CEC Survey",2017,15,"I",288.25346306385967,"TON",8,{"v":0.180819577782,"d":"0.18"},{"$f":"VLOOKUP(A461,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.14697194,"d":"0.15"}]
["01061","01","AL","061","Geneva","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",409.450314455,"A","CEC Survey",2017,15,"I",79.09819685091625,"TON",8,{"v":0.193181429,"d":"0.19"},{"$f":"VLOOKUP(A462,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.15701977485166219,"d":"0.16"}]
["01061","01","AL","061","Geneva","","2104009000","Wax Log; Total: All Combustor Types",null,153.58326148495638,"A","CEC Survey",2017,15,"I",35.95880225297425,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A463,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.1903050475493782,"d":"0.19"}]
["01061","01","AL","061","Geneva","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",441.30440516423994,"A","CEC Survey",2017,15,"I",392.82810709694365,"TON",8,{"v":0.8901522452529,"d":"0.89"},{"$f":"VLOOKUP(A464,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.723524543,"d":"0.72"}]
["01061","01","AL","061","Geneva","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",583.6606648946399,"A","CEC Survey",2017,15,"I",519.5468513217642,"TON",8,{"v":0.8901522452528999,"d":"0.89"},{"$f":"VLOOKUP(A465,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.723524543,"d":"0.72"}]
["01061","01","AL","061","Geneva","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",398.59752724512,"A","CEC Survey",2017,15,"I",354.8124838294975,"TON",8,{"v":0.8901522452529,"d":"0.89"},{"$f":"VLOOKUP(A466,cordwood_density!A:D,4,FALSE)","v":1.2303},{"v":0.723524543,"d":"0.72"}]
["01063","01","AL","063","Greene","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",15.47714515559788,"A","CEC Survey",2017,15,"I",25.53429364651968,"TON",8,{"v":1.649806433280382,"d":"1.65"},{"$f":"VLOOKUP(A467,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":1.2661599641445755,"d":"1.27"}]
["01063","01","AL","063","Greene","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.2549036612646929,"A","CEC Survey",2017,15,"I",2.0703481335015956,"TON",8,{"v":1.649806433280382,"d":"1.65"},{"$f":"VLOOKUP(A468,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":1.2661599641445755,"d":"1.27"}]
["01063","01","AL","063","Greene","","2104008610","Hydronic heater: outdoor","Hydronic heater",15.058843935176315,"A","CEC Survey",2017,15,"I",24.844177602019144,"TON",8,{"v":1.6498064332803817,"d":"1.65"},{"$f":"VLOOKUP(A469,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":1.2661599641445753,"d":"1.27"}]
["01063","01","AL","063","Greene","","2104008620","Hydronic heater: indoor","Hydronic heater",9.62092806969598,"A","CEC Survey",2017,15,"I",15.872669023512232,"TON",8,{"v":1.6498064332803817,"d":"1.65"},{"$f":"VLOOKUP(A470,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":1.2661599641445753,"d":"1.27"}]
["01063","01","AL","063","Greene","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.4183012204215643,"A","CEC Survey",2017,15,"I",0.6901160445005319,"TON",8,{"v":1.649806433280382,"d":"1.65"},{"$f":"VLOOKUP(A471,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":1.2661599641445755,"d":"1.27"}]
["01063","01","AL","063","Greene","","2104008100","Fireplace: general","Fireplace: general",248.69776745000001,"A","CEC Survey",2017,15,"I",69.95584782641411,"TON",8,{"v":0.28128860401,"d":"0.28"},{"$f":"VLOOKUP(A472,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.21587767000000002,"d":"0.22"}]
["01063","01","AL","063","Greene","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",88.44365775025,"A","CEC Survey",2017,15,"I",46.951546941764185,"TON",8,{"v":0.5308639210099999,"d":"0.53"},{"$f":"VLOOKUP(A473,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.4074166699999999,"d":"0.41"}]
["01063","01","AL","063","Greene","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",116.97386992774999,"A","CEC Survey",2017,15,"I",62.097207245559076,"TON",8,{"v":0.5308639210099999,"d":"0.53"},{"$f":"VLOOKUP(A474,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.4074166699999999,"d":"0.41"}]
["01063","01","AL","063","Greene","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",79.884594097,"A","CEC Survey",2017,15,"I",42.40784885062572,"TON",8,{"v":0.5308639210099999,"d":"0.53"},{"$f":"VLOOKUP(A475,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.4074166699999999,"d":"0.41"}]
["01063","01","AL","063","Greene","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,405.18934527500005,"A","CEC Survey",2017,15,"I",77.98094290482732,"TON",8,{"v":0.19245556136699998,"d":"0.19"},{"$f":"VLOOKUP(A476,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.147701889,"d":"0.15"}]
["01063","01","AL","063","Greene","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",100.08082425,"A","CEC Survey",2017,15,"I",26.749250020715344,"TON",8,{"v":0.267276476,"d":"0.27"},{"$f":"VLOOKUP(A477,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.205123926323868,"d":"0.21"}]
["01063","01","AL","063","Greene","","2104009000","Wax Log; Total: All Combustor Types",null,43.44799083437698,"A","CEC Survey",2017,15,"I",10.172578024431601,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A478,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.17968710667689947,"d":"0.18"}]
["01063","01","AL","063","Greene","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",123.7853912625,"A","CEC Survey",2017,15,"I",128.66214714511267,"TON",8,{"v":1.0393968612359998,"d":"1.04"},{"$f":"VLOOKUP(A479,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.7976952119999999,"d":"0.80"}]
["01063","01","AL","063","Greene","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",163.7161626375,"A","CEC Survey",2017,15,"I",170.16606557901997,"TON",8,{"v":1.0393968612359998,"d":"1.04"},{"$f":"VLOOKUP(A480,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.7976952119999999,"d":"0.80"}]
["01063","01","AL","063","Greene","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",111.80615985000001,"A","CEC Survey",2017,15,"I",116.21097161494049,"TON",8,{"v":1.0393968612359998,"d":"1.04"},{"$f":"VLOOKUP(A481,cordwood_density!A:D,4,FALSE)","v":1.303},{"v":0.7976952119999999,"d":"0.80"}]
["01065","01","AL","065","Hale","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",27.49299936223041,"A","CEC Survey",2017,15,"I",46.228415565688906,"TON",8,{"v":1.6814613406348458,"d":"1.68"},{"$f":"VLOOKUP(A482,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":1.2279714749396375,"d":"1.23"}]
["01065","01","AL","065","Hale","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.229162110451114,"A","CEC Survey",2017,15,"I",3.748249910731533,"TON",8,{"v":1.681461340634846,"d":"1.68"},{"$f":"VLOOKUP(A483,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":1.2279714749396378,"d":"1.23"}]
["01065","01","AL","065","Hale","","2104008610","Hydronic heater: outdoor","Hydronic heater",26.74994532541337,"A","CEC Survey",2017,15,"I",44.978998928778395,"TON",8,{"v":1.6814613406348458,"d":"1.68"},{"$f":"VLOOKUP(A484,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":1.2279714749396375,"d":"1.23"}]
["01065","01","AL","065","Hale","","2104008620","Hydronic heater: indoor","Hydronic heater",17.090242846791877,"A","CEC Survey",2017,15,"I",28.736582648941756,"TON",8,{"v":1.681461340634846,"d":"1.68"},{"$f":"VLOOKUP(A485,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":1.2279714749396378,"d":"1.23"}]
["01065","01","AL","065","Hale","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7430540368170381,"A","CEC Survey",2017,15,"I",1.249416636910511,"TON",8,{"v":1.681461340634846,"d":"1.68"},{"$f":"VLOOKUP(A486,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":1.2279714749396378,"d":"1.23"}]
["01065","01","AL","065","Hale","","2104008100","Fireplace: general","Fireplace: general",500.403066336,"A","CEC Survey",2017,15,"I",149.10155938943495,"TON",8,{"v":0.29796292113309997,"d":"0.30"},{"$f":"VLOOKUP(A487,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.217602367,"d":"0.22"}]
["01065","01","AL","065","Hale","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",157.51917887136,"A","CEC Survey",2017,15,"I",84.10766215761986,"TON",8,{"v":0.5339518829406,"d":"0.53"},{"$f":"VLOOKUP(A488,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.389945142,"d":"0.39"}]
["01065","01","AL","065","Hale","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",208.33181721696,"A","CEC Survey",2017,15,"I",111.2391660794327,"TON",8,{"v":0.5339518829406,"d":"0.53"},{"$f":"VLOOKUP(A489,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.389945142,"d":"0.39"}]
["01065","01","AL","065","Hale","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",142.27538736768,"A","CEC Survey",2017,15,"I",75.968210981076,"TON",8,{"v":0.5339518829406,"d":"0.53"},{"$f":"VLOOKUP(A490,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.389945142,"d":"0.39"}]
["01065","01","AL","065","Hale","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,795.8623582079999,"A","CEC Survey",2017,15,"I",160.72641390461854,"TON",8,{"v":0.2019525263973,"d":"0.20"},{"$f":"VLOOKUP(A491,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.147485961,"d":"0.15"}]
["01065","01","AL","065","Hale","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",195.41331849600002,"A","CEC Survey",2017,15,"I",45.643837049770205,"TON",8,{"v":0.233575876,"d":"0.23"},{"$f":"VLOOKUP(A492,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.1705804980647046,"d":"0.17"}]
["01065","01","AL","065","Hale","","2104009000","Wax Log; Total: All Combustor Types",null,81.35187440856569,"A","CEC Survey",2017,15,"I",19.047101464588625,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A493,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.17098685459723947,"d":"0.17"}]
["01065","01","AL","065","Hale","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",217.62330103872,"A","CEC Survey",2017,15,"I",228.86186050221775,"TON",8,{"v":1.0516422616964998,"d":"1.05"},{"$f":"VLOOKUP(A494,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.7680145049999999,"d":"0.77"}]
["01065","01","AL","065","Hale","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",287.82436588992,"A","CEC Survey",2017,15,"I",302.68826711583637,"TON",8,{"v":1.0516422616964998,"d":"1.05"},{"$f":"VLOOKUP(A495,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.7680145049999999,"d":"0.77"}]
["01065","01","AL","065","Hale","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",196.56298158336003,"A","CEC Survey",2017,15,"I",206.71393851813218,"TON",8,{"v":1.0516422616964998,"d":"1.05"},{"$f":"VLOOKUP(A496,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.7680145049999999,"d":"0.77"}]
["01067","01","AL","067","Henry","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",32.59988695330765,"A","CEC Survey",2017,15,"I",53.10429732718112,"TON",8,{"v":1.6289718244496258,"d":"1.63"},{"$f":"VLOOKUP(A497,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":1.1939982587771207,"d":"1.19"}]
["01067","01","AL","067","Henry","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.6432340772952148,"A","CEC Survey",2017,15,"I",4.30575383733901,"TON",8,{"v":1.628971824449626,"d":"1.63"},{"$f":"VLOOKUP(A498,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":1.193998258777121,"d":"1.19"}]
["01067","01","AL","067","Henry","","2104008610","Hydronic heater: outdoor","Hydronic heater",31.71880892754258,"A","CEC Survey",2017,15,"I",51.66904604806812,"TON",8,{"v":1.6289718244496258,"d":"1.63"},{"$f":"VLOOKUP(A499,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":1.1939982587771207,"d":"1.19"}]
["01067","01","AL","067","Henry","","2104008620","Hydronic heater: indoor","Hydronic heater",20.26479459259665,"A","CEC Survey",2017,15,"I",33.010779419599075,"TON",8,{"v":1.6289718244496256,"d":"1.63"},{"$f":"VLOOKUP(A500,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":1.1939982587771205,"d":"1.19"}]
["01067","01","AL","067","Henry","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8810780257650717,"A","CEC Survey",2017,15,"I",1.4352512791130034,"TON",8,{"v":1.628971824449626,"d":"1.63"},{"$f":"VLOOKUP(A501,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":1.193998258777121,"d":"1.19"}]
["01067","01","AL","067","Henry","","2104008100","Fireplace: general","Fireplace: general",507.993595921,"A","CEC Survey",2017,15,"I",156.9111398400332,"TON",8,{"v":0.3088840904688,"d":"0.31"},{"$f":"VLOOKUP(A502,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.22640481599999998,"d":"0.23"}]
["01067","01","AL","067","Henry","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",202.23199015887,"A","CEC Survey",2017,15,"I",101.13121758541769,"TON",8,{"v":0.5000752724925999,"d":"0.50"},{"$f":"VLOOKUP(A503,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.36654348199999987,"d":"0.37"}]
["01067","01","AL","067","Henry","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",267.46811601657,"A","CEC Survey",2017,15,"I",133.75419100006854,"TON",8,{"v":0.5000752724925999,"d":"0.50"},{"$f":"VLOOKUP(A504,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.36654348199999987,"d":"0.37"}]
["01067","01","AL","067","Henry","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",182.66115240156,"A","CEC Survey",2017,15,"I",91.34432556102244,"TON",8,{"v":0.5000752724926,"d":"0.50"},{"$f":"VLOOKUP(A505,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.366543482,"d":"0.37"}]
["01067","01","AL","067","Henry","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1038.573027072,"A","CEC Survey",2017,15,"I",207.72950918721918,"TON",8,{"v":0.20001435024060002,"d":"0.20"},{"$f":"VLOOKUP(A506,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.14660584200000001,"d":"0.15"}]
["01067","01","AL","067","Henry","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",263.041387364,"A","CEC Survey",2017,15,"I",54.09128403448863,"TON",8,{"v":0.205637921,"d":"0.21"},{"$f":"VLOOKUP(A507,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.15072778787656674,"d":"0.15"}]
["01067","01","AL","067","Henry","","2104009000","Wax Log; Total: All Combustor Types",null,96.61971383234841,"A","CEC Survey",2017,15,"I",22.621795824909547,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A508,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.1716135014293044,"d":"0.17"}]
["01067","01","AL","067","Henry","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",280.46017884633,"A","CEC Survey",2017,15,"I",279.58486491592043,"TON",8,{"v":0.9968790081572002,"d":"1.00"},{"$f":"VLOOKUP(A509,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.7306890040000001,"d":"0.73"}]
["01067","01","AL","067","Henry","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",370.93120428062997,"A","CEC Survey",2017,15,"I",369.77353101783024,"TON",8,{"v":0.9968790081572002,"d":"1.00"},{"$f":"VLOOKUP(A510,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.7306890040000001,"d":"0.73"}]
["01067","01","AL","067","Henry","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",253.31887121604,"A","CEC Survey",2017,15,"I",252.5282650853475,"TON",8,{"v":0.9968790081572002,"d":"1.00"},{"$f":"VLOOKUP(A511,cordwood_density!A:D,4,FALSE)","v":1.3643},{"v":0.7306890040000001,"d":"0.73"}]
["01069","01","AL","069","Houston","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",102.74960546533477,"A","CEC Survey",2017,15,"I",145.84582466868704,"TON",8,{"v":1.4194295346262122,"d":"1.42"},{"$f":"VLOOKUP(A512,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":1.169795232096763,"d":"1.17"}]
["01069","01","AL","069","Houston","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.3310490917839,"A","CEC Survey",2017,15,"I",11.82533713529895,"TON",8,{"v":1.4194295346262125,"d":"1.42"},{"$f":"VLOOKUP(A513,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":1.169795232096763,"d":"1.17"}]
["01069","01","AL","069","Houston","","2104008610","Hydronic heater: outdoor","Hydronic heater",99.9725891014068,"A","CEC Survey",2017,15,"I",141.9040456235874,"TON",8,{"v":1.4194295346262122,"d":"1.42"},{"$f":"VLOOKUP(A514,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":1.169795232096763,"d":"1.17"}]
["01069","01","AL","069","Houston","","2104008620","Hydronic heater: indoor","Hydronic heater",63.871376370343235,"A","CEC Survey",2017,15,"I",90.66091803729195,"TON",8,{"$f":"P515/J515","v":{"v":1.4194295346262122,"d":"1.42"}},{"$f":"VLOOKUP(A515,cordwood_density!A:D,4,FALSE)","v":1.2134},{"$f":"S515/T515","v":{"v":1.169795232096763,"d":"1.17"}}]
["01069","01","AL","069","Houston","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.7770163639279666,"A","CEC Survey",2017,15,"I",3.94177904509965,"TON",8,{"v":1.4194295346262125,"d":"1.42"},{"$f":"VLOOKUP(A516,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":1.169795232096763,"d":"1.17"}]
["01069","01","AL","069","Houston","","2104008100","Fireplace: general","Fireplace: general",2630.21519704,"A","CEC Survey",2017,15,"I",615.8149430406379,"TON",8,{"v":0.2341310109278,"d":"0.23"},{"$f":"VLOOKUP(A517,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.192954517,"d":"0.19"}]
["01069","01","AL","069","Houston","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",983.8074900908,"A","CEC Survey",2017,15,"I",380.1075764523109,"TON",8,{"v":0.3863637757192,"d":"0.39"},{"$f":"VLOOKUP(A518,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.318414188,"d":"0.32"}]
["01069","01","AL","069","Houston","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1301.1647449588,"A","CEC Survey",2017,15,"I",502.72292369499183,"TON",8,{"v":0.3863637757192,"d":"0.39"},{"$f":"VLOOKUP(A519,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.318414188,"d":"0.32"}]
["01069","01","AL","069","Houston","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",888.6003136304001,"A","CEC Survey",2017,15,"I",343.3229722795067,"TON",8,{"v":0.3863637757192,"d":"0.39"},{"$f":"VLOOKUP(A520,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.318414188,"d":"0.32"}]
["01069","01","AL","069","Houston","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5308.604861,"A","CEC Survey",2017,15,"I",950.5424257417097,"TON",8,{"v":0.179056918085,"d":"0.18"},{"$f":"VLOOKUP(A521,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.147566275,"d":"0.15"}]
["01069","01","AL","069","Houston","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1151.49186924,"A","CEC Survey",2017,15,"I",173.94261840870436,"TON",8,{"v":0.151058486,"d":"0.15"},{"$f":"VLOOKUP(A522,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.12449191198285807,"d":"0.12"}]
["01069","01","AL","069","Houston","","2104009000","Wax Log; Total: All Combustor Types",null,568.1991793084144,"A","CEC Survey",2017,15,"I",133.03378070959147,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A523,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.1929555793637712,"d":"0.19"}]
["01069","01","AL","069","Houston","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1126.6598507368,"A","CEC Survey",2017,15,"I",814.2002858917209,"TON",8,{"v":0.7226673475221999,"d":"0.72"},{"$f":"VLOOKUP(A524,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.5955722329999998,"d":"0.60"}]
["01069","01","AL","069","Houston","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1490.0985122647999,"A","CEC Survey",2017,15,"I",1076.8455394051794,"TON",8,{"v":0.7226673475222,"d":"0.72"},{"$f":"VLOOKUP(A525,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.595572233,"d":"0.60"}]
["01069","01","AL","069","Houston","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1017.6282522784002,"A","CEC Survey",2017,15,"I",735.4067098376835,"TON",8,{"v":0.7226673475221999,"d":"0.72"},{"$f":"VLOOKUP(A526,cordwood_density!A:D,4,FALSE)","v":1.2134},{"v":0.5955722329999998,"d":"0.60"}]
["01071","01","AL","071","Jackson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",132.52069907023093,"A","CEC Survey",2017,15,"I",233.5367274969557,"TON",8,{"v":1.7622660394599194,"d":"1.76"},{"$f":"VLOOKUP(A527,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":1.258312059592945,"d":"1.26"}]
["01071","01","AL","071","Jackson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.74492154623494,"A","CEC Survey",2017,15,"I",18.935410337591005,"TON",8,{"v":1.7622660394599199,"d":"1.76"},{"$f":"VLOOKUP(A528,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":1.2583120595929451,"d":"1.26"}]
["01071","01","AL","071","Jackson","","2104008610","Hydronic heater: outdoor","Hydronic heater",128.93905855481927,"A","CEC Survey",2017,15,"I",227.22492405109205,"TON",8,{"v":1.7622660394599199,"d":"1.76"},{"$f":"VLOOKUP(A529,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":1.2583120595929451,"d":"1.26"}]
["01071","01","AL","071","Jackson","","2104008620","Hydronic heater: indoor","Hydronic heater",82.37773185446788,"A","CEC Survey",2017,15,"I",145.17147925486438,"TON",8,{"v":1.7622660394599197,"d":"1.76"},{"$f":"VLOOKUP(A530,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":1.2583120595929451,"d":"1.26"}]
["01071","01","AL","071","Jackson","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.581640515411647,"A","CEC Survey",2017,15,"I",6.311803445863668,"TON",8,{"v":1.7622660394599197,"d":"1.76"},{"$f":"VLOOKUP(A531,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":1.2583120595929451,"d":"1.26"}]
["01071","01","AL","071","Jackson","","2104008100","Fireplace: general","Fireplace: general",1940.92904608,"A","CEC Survey",2017,15,"I",563.9916780093772,"TON",8,{"v":0.29057820488,"d":"0.29"},{"$f":"VLOOKUP(A532,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.20748176000000002,"d":"0.21"}]
["01071","01","AL","071","Jackson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",591.21743487568,"A","CEC Survey",2017,15,"I",335.6880188244465,"TON",8,{"v":0.567791135752,"d":"0.57"},{"$f":"VLOOKUP(A533,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.405420304,"d":"0.41"}]
["01071","01","AL","071","Jackson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",781.93273644848,"A","CEC Survey",2017,15,"I",443.9744765097518,"TON",8,{"v":0.5677911357520001,"d":"0.57"},{"$f":"VLOOKUP(A534,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.40542030400000006,"d":"0.41"}]
["01071","01","AL","071","Jackson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",534.0028444038401,"A","CEC Survey",2017,15,"I",303.2020815188549,"TON",8,{"v":0.567791135752,"d":"0.57"},{"$f":"VLOOKUP(A535,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.405420304,"d":"0.41"}]
["01071","01","AL","071","Jackson","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3178.626841488,"A","CEC Survey",2017,15,"I",653.014753666367,"TON",8,{"v":0.20543926237050003,"d":"0.21"},{"$f":"VLOOKUP(A536,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.14668994100000002,"d":"0.15"}]
["01071","01","AL","071","Jackson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",781.144737024,"A","CEC Survey",2017,15,"I",224.6730945422903,"TON",8,{"v":0.287620314,"d":"0.29"},{"$f":"VLOOKUP(A537,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.20536973509460904,"d":"0.21"}]
["01071","01","AL","071","Jackson","","2104009000","Wax Log; Total: All Combustor Types",null,292.54501729407946,"A","CEC Survey",2017,15,"I",100.4683696080341,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A538,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.24521867190289182,"d":"0.25"}]
["01071","01","AL","071","Jackson","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",886.9583281071999,"A","CEC Survey",2017,15,"I",931.4203845743639,"TON",8,{"v":1.0501286870625,"d":"1.05"},{"$f":"VLOOKUP(A539,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.749824125,"d":"0.75"}]
["01071","01","AL","071","Jackson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1173.0739178191998,"A","CEC Survey",2017,15,"I",1231.8785731467392,"TON",8,{"v":1.0501286870625,"d":"1.05"},{"$f":"VLOOKUP(A540,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.749824125,"d":"0.75"}]
["01071","01","AL","071","Jackson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",801.1236511936,"A","CEC Survey",2017,15,"I",841.2829280026514,"TON",8,{"v":1.0501286870625,"d":"1.05"},{"$f":"VLOOKUP(A541,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":0.749824125,"d":"0.75"}]
["01073","01","AL","073","Jefferson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",701.4693603287872,"A","CEC Survey",2017,15,"I",1025.5390591246196,"TON",8,{"v":1.4619869621161172,"d":"1.46"},{"$f":"VLOOKUP(A542,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":1.083997154382826,"d":"1.08"}]
["01073","01","AL","073","Jefferson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",56.87589408071247,"A","CEC Survey",2017,15,"I",83.1518156046989,"TON",8,{"v":1.4619869621161174,"d":"1.46"},{"$f":"VLOOKUP(A543,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":1.083997154382826,"d":"1.08"}]
["01073","01","AL","073","Jefferson","","2104008610","Hydronic heater: outdoor","Hydronic heater",682.5107289685496,"A","CEC Survey",2017,15,"I",997.8217872563868,"TON",8,{"v":1.4619869621161174,"d":"1.46"},{"$f":"VLOOKUP(A544,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":1.083997154382826,"d":"1.08"}]
["01073","01","AL","073","Jefferson","","2104008620","Hydronic heater: indoor","Hydronic heater",436.0485212854623,"A","CEC Survey",2017,15,"I",637.4972529693582,"TON",8,{"v":1.4619869621161174,"d":"1.46"},{"$f":"VLOOKUP(A545,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":1.083997154382826,"d":"1.08"}]
["01073","01","AL","073","Jefferson","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",18.95863136023749,"A","CEC Survey",2017,15,"I",27.717271868232967,"TON",8,{"v":1.4619869621161177,"d":"1.46"},{"$f":"VLOOKUP(A546,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":1.0839971543828262,"d":"1.08"}]
["01073","01","AL","073","Jefferson","","2104008100","Fireplace: general","Fireplace: general",45959.48278638,"A","CEC Survey",2017,15,"I",8771.991297125396,"TON",8,{"v":0.1908635773361,"d":"0.19"},{"$f":"VLOOKUP(A547,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.141516703,"d":"0.14"}]
["01073","01","AL","073","Jefferson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",4675.1947030887,"A","CEC Survey",2017,15,"I",2900.6621938676044,"TON",8,{"v":0.62043666159,"d":"0.62"},{"$f":"VLOOKUP(A548,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.4600257,"d":"0.46"}]
["01073","01","AL","073","Jefferson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6183.3220266657,"A","CEC Survey",2017,15,"I",3836.3596757603796,"TON",8,{"v":0.62043666159,"d":"0.62"},{"$f":"VLOOKUP(A549,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.4600257,"d":"0.46"}]
["01073","01","AL","073","Jefferson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",4222.7565060156,"A","CEC Survey",2017,15,"I",2619.952949299772,"TON",8,{"v":0.6204366615900001,"d":"0.62"},{"$f":"VLOOKUP(A550,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.4600257000000001,"d":"0.46"}]
["01073","01","AL","073","Jefferson","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,32352.1723386,"A","CEC Survey",2017,15,"I",6818.079810847639,"TON",8,{"v":0.21074565687550004,"d":"0.21"},{"$f":"VLOOKUP(A551,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.15625836500000004,"d":"0.16"}]
["01073","01","AL","073","Jefferson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",6313.81140945,"A","CEC Survey",2017,15,"I",1406.9676256688272,"TON",8,{"v":0.222839666,"d":"0.22"},{"$f":"VLOOKUP(A552,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.16522552532067916,"d":"0.17"}]
["01073","01","AL","073","Jefferson","","2104009000","Wax Log; Total: All Combustor Types",null,1704.2236071834002,"A","CEC Survey",2017,15,"I",585.2793831354861,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A553,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.2546368725439312,"d":"0.25"}]
["01073","01","AL","073","Jefferson","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",5062.982012353499,"A","CEC Survey",2017,15,"I",3741.740369280256,"TON",8,{"v":0.7390388431463,"d":"0.74"},{"$f":"VLOOKUP(A554,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.547963849,"d":"0.55"}]
["01073","01","AL","073","Jefferson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6696.202016338499,"A","CEC Survey",2017,15,"I",4948.753391628726,"TON",8,{"v":0.7390388431463001,"d":"0.74"},{"$f":"VLOOKUP(A555,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.5479638490000001,"d":"0.55"}]
["01073","01","AL","073","Jefferson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",4573.016011158,"A","CEC Survey",2017,15,"I",3379.6364625757155,"TON",8,{"v":0.7390388431463,"d":"0.74"},{"$f":"VLOOKUP(A556,cordwood_density!A:D,4,FALSE)","v":1.3487},{"v":0.547963849,"d":"0.55"}]
["01075","01","AL","075","Lamar","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",45.425059115202465,"A","CEC Survey",2017,15,"I",69.9478346640154,"TON",8,{"v":1.5398512632998616,"d":"1.54"},{"$f":"VLOOKUP(A557,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":1.1795107340481512,"d":"1.18"}]
["01075","01","AL","075","Lamar","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.6831129012326325,"A","CEC Survey",2017,15,"I",5.6714460538390865,"TON",8,{"v":1.5398512632998613,"d":"1.54"},{"$f":"VLOOKUP(A558,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":1.179510734048151,"d":"1.18"}]
["01075","01","AL","075","Lamar","","2104008610","Hydronic heater: outdoor","Hydronic heater",44.19735481479159,"A","CEC Survey",2017,15,"I",68.05735264606903,"TON",8,{"v":1.5398512632998613,"d":"1.54"},{"$f":"VLOOKUP(A559,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":1.179510734048151,"d":"1.18"}]
["01075","01","AL","075","Lamar","","2104008620","Hydronic heater: indoor","Hydronic heater",28.237198909450182,"A","CEC Survey",2017,15,"I",43.48108641276633,"TON",8,{"v":1.5398512632998613,"d":"1.54"},{"$f":"VLOOKUP(A560,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":1.179510734048151,"d":"1.18"}]
["01075","01","AL","075","Lamar","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2277043004108774,"A","CEC Survey",2017,15,"I",1.8904820179463622,"TON",8,{"v":1.5398512632998613,"d":"1.54"},{"$f":"VLOOKUP(A561,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":1.179510734048151,"d":"1.18"}]
["01075","01","AL","075","Lamar","","2104008100","Fireplace: general","Fireplace: general",792.97152987,"A","CEC Survey",2017,15,"I",222.2210077411575,"TON",8,{"v":0.28023831798550003,"d":"0.28"},{"$f":"VLOOKUP(A562,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.214659761,"d":"0.21"}]
["01075","01","AL","075","Lamar","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",168.81888498137002,"A","CEC Survey",2017,15,"I",109.72748645294308,"TON",8,{"v":0.6499716335945,"d":"0.65"},{"$f":"VLOOKUP(A563,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.497871799,"d":"0.50"}]
["01075","01","AL","075","Lamar","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",223.27658981407,"A","CEC Survey",2017,15,"I",145.1234498248602,"TON",8,{"v":0.6499716335945,"d":"0.65"},{"$f":"VLOOKUP(A564,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.497871799,"d":"0.50"}]
["01075","01","AL","075","Lamar","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",152.48157353156003,"A","CEC Survey",2017,15,"I",99.10869744136795,"TON",8,{"v":0.6499716335945,"d":"0.65"},{"$f":"VLOOKUP(A565,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.497871799,"d":"0.50"}]
["01075","01","AL","075","Lamar","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,970.7245596230001,"A","CEC Survey",2017,15,"I",183.87957101601296,"TON",8,{"v":0.18942507346,"d":"0.19"},{"$f":"VLOOKUP(A566,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.14509771999999999,"d":"0.15"}]
["01075","01","AL","075","Lamar","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",246.198479488,"A","CEC Survey",2017,15,"I",74.69432681501364,"TON",8,{"v":0.303390691,"d":"0.30"},{"$f":"VLOOKUP(A567,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.23239424818077362,"d":"0.23"}]
["01075","01","AL","075","Lamar","","2104009000","Wax Log; Total: All Combustor Types",null,86.4507295312777,"A","CEC Survey",2017,15,"I",29.68966597951479,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A568,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.2630630026809651,"d":"0.26"}]
["01075","01","AL","075","Lamar","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",256.19916487698003,"A","CEC Survey",2017,15,"I",270.788141662363,"TON",8,{"v":1.0569438889170002,"d":"1.06"},{"$f":"VLOOKUP(A569,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.8096084940000001,"d":"0.81"}]
["01075","01","AL","075","Lamar","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",338.84405677278,"A","CEC Survey",2017,15,"I",358.1391551018349,"TON",8,{"v":1.0569438889170002,"d":"1.06"},{"$f":"VLOOKUP(A570,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.8096084940000001,"d":"0.81"}]
["01075","01","AL","075","Lamar","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",231.40569730824004,"A","CEC Survey",2017,15,"I",244.58283763052142,"TON",8,{"v":1.0569438889170002,"d":"1.06"},{"$f":"VLOOKUP(A571,cordwood_density!A:D,4,FALSE)","v":1.3055},{"v":0.8096084940000001,"d":"0.81"}]
["01077","01","AL","077","Lauderdale","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",161.2395097052658,"A","CEC Survey",2017,15,"I",274.5910347955775,"TON",8,{"v":1.7030009288511863,"d":"1.70"},{"$f":"VLOOKUP(A572,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":1.2160817829557171,"d":"1.22"}]
["01077","01","AL","077","Lauderdale","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.073473759886415,"A","CEC Survey",2017,15,"I",22.264137956398173,"TON",8,{"v":1.703000928851186,"d":"1.70"},{"$f":"VLOOKUP(A573,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":1.216081782955717,"d":"1.22"}]
["01077","01","AL","077","Lauderdale","","2104008610","Hydronic heater: outdoor","Hydronic heater",156.88168511863697,"A","CEC Survey",2017,15,"I",267.1696554767781,"TON",8,{"v":1.7030009288511863,"d":"1.70"},{"$f":"VLOOKUP(A574,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":1.2160817829557171,"d":"1.22"}]
["01077","01","AL","077","Lauderdale","","2104008620","Hydronic heater: indoor","Hydronic heater",100.22996549246253,"A","CEC Survey",2017,15,"I",170.69172433238603,"TON",8,{"v":1.7030009288511863,"d":"1.70"},{"$f":"VLOOKUP(A575,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":1.2160817829557171,"d":"1.22"}]
["01077","01","AL","077","Lauderdale","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.357824586628805,"A","CEC Survey",2017,15,"I",7.421379318799392,"TON",8,{"v":1.7030009288511863,"d":"1.70"},{"$f":"VLOOKUP(A576,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":1.2160817829557171,"d":"1.22"}]
["01077","01","AL","077","Lauderdale","","2104008100","Fireplace: general","Fireplace: general",3327.3384136827535,"A","CEC Survey",2017,15,"I",910.0307723001046,"TON",8,{"v":0.27350111685600004,"d":"0.27"},{"$f":"VLOOKUP(A577,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.19530214,"d":"0.20"}]
["01077","01","AL","077","Lauderdale","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",820.2085750247777,"A","CEC Survey",2017,15,"I",373.09381918594966,"TON",8,{"v":0.4548767600664,"d":"0.45"},{"$f":"VLOOKUP(A578,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.324819166,"d":"0.32"}]
["01077","01","AL","077","Lauderdale","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1084.791986323093,"A","CEC Survey",2017,15,"I",493.44666408464303,"TON",8,{"$f":"P579/J579","v":{"v":0.4548767600664,"d":"0.45"}},{"$f":"VLOOKUP(A579,cordwood_density!A:D,4,FALSE)","v":1.4004},{"$f":"S579/T579","v":{"v":0.324819166,"d":"0.32"}}]
["01077","01","AL","077","Lauderdale","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",740.8335516352831,"A","CEC Survey",2017,15,"I",336.98796571634165,"TON",8,{"v":0.4548767600664,"d":"0.45"},{"$f":"VLOOKUP(A580,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.324819166,"d":"0.32"}]
["01077","01","AL","077","Lauderdale","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5411.447959149304,"A","CEC Survey",2017,15,"I",1120.1257889934896,"TON",8,{"v":0.2069918804448,"d":"0.21"},{"$f":"VLOOKUP(A581,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.147809112,"d":"0.15"}]
["01077","01","AL","077","Lauderdale","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1269.7426869973403,"A","CEC Survey",2017,15,"I",254.68666929724412,"TON",8,{"v":0.200581324,"d":"0.20"},{"$f":"VLOOKUP(A582,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.143231451013996,"d":"0.14"}]
["01077","01","AL","077","Lauderdale","","2104009000","Wax Log; Total: All Combustor Types",null,554.8990669292034,"A","CEC Survey",2017,15,"I",190.56829293166265,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A583,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.2452361825192802,"d":"0.25"}]
["01077","01","AL","077","Lauderdale","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1197.5527739739462,"A","CEC Survey",2017,15,"I",1095.85170086342,"TON",8,{"v":0.9150759153828,"d":"0.92"},{"$f":"VLOOKUP(A584,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.653438957,"d":"0.65"}]
["01077","01","AL","077","Lauderdale","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1583.8601204171543,"A","CEC Survey",2017,15,"I",1449.3522495290395,"TON",8,{"v":0.9150759153828001,"d":"0.92"},{"$f":"VLOOKUP(A585,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.653438957,"d":"0.65"}]
["01077","01","AL","077","Lauderdale","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1081.6605700409837,"A","CEC Survey",2017,15,"I",989.8015362637344,"TON",8,{"v":0.9150759153828001,"d":"0.92"},{"$f":"VLOOKUP(A586,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.653438957,"d":"0.65"}]
["01079","01","AL","079","Lawrence","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",86.48130157124861,"A","CEC Survey",2017,15,"I",139.71375785806163,"TON",8,{"v":1.6155371776285865,"d":"1.62"},{"$f":"VLOOKUP(A587,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":1.2716759899469352,"d":"1.27"}]
["01079","01","AL","079","Lawrence","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.011997424695832,"A","CEC Survey",2017,15,"I",11.328142529032025,"TON",8,{"v":1.615537177628587,"d":"1.62"},{"$f":"VLOOKUP(A588,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":1.2716759899469356,"d":"1.27"}]
["01079","01","AL","079","Lawrence","","2104008610","Hydronic heater: outdoor","Hydronic heater",84.14396909634999,"A","CEC Survey",2017,15,"I",135.9377103483843,"TON",8,{"v":1.6155371776285867,"d":"1.62"},{"$f":"VLOOKUP(A589,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":1.2716759899469354,"d":"1.27"}]
["01079","01","AL","079","Lawrence","","2104008620","Hydronic heater: indoor","Hydronic heater",53.758646922668056,"A","CEC Survey",2017,15,"I",86.84909272257886,"TON",8,{"v":1.6155371776285867,"d":"1.62"},{"$f":"VLOOKUP(A590,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":1.2716759899469354,"d":"1.27"}]
["01079","01","AL","079","Lawrence","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.337332474898611,"A","CEC Survey",2017,15,"I",3.776047509677342,"TON",8,{"v":1.6155371776285867,"d":"1.62"},{"$f":"VLOOKUP(A591,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":1.2716759899469354,"d":"1.27"}]
["01079","01","AL","079","Lawrence","","2104008100","Fireplace: general","Fireplace: general",1026.1984012799999,"A","CEC Survey",2017,15,"I",290.6219315643318,"TON",8,{"v":0.2832024793664,"d":"0.28"},{"$f":"VLOOKUP(A592,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.22292386599999997,"d":"0.22"}]
["01079","01","AL","079","Lawrence","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",346.34469275903996,"A","CEC Survey",2017,15,"I",147.65585967981318,"TON",8,{"v":0.4263263239392,"d":"0.43"},{"$f":"VLOOKUP(A593,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.335584323,"d":"0.34"}]
["01079","01","AL","079","Lawrence","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",458.0687871974399,"A","CEC Survey",2017,15,"I",195.28678215717227,"TON",8,{"v":0.42632632393920006,"d":"0.43"},{"$f":"VLOOKUP(A594,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.3355843230000001,"d":"0.34"}]
["01079","01","AL","079","Lawrence","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",312.82746442752,"A","CEC Survey",2017,15,"I",133.36658293660548,"TON",8,{"v":0.42632632393920006,"d":"0.43"},{"$f":"VLOOKUP(A595,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.3355843230000001,"d":"0.34"}]
["01079","01","AL","079","Lawrence","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2030.745502464,"A","CEC Survey",2017,15,"I",381.68558547198,"TON",8,{"v":0.187953431392,"d":"0.19"},{"$f":"VLOOKUP(A596,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.14794823,"d":"0.15"}]
["01079","01","AL","079","Lawrence","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",539.394134784,"A","CEC Survey",2017,15,"I",138.1878429541158,"TON",8,{"v":0.256190852,"d":"0.26"},{"$f":"VLOOKUP(A597,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.20166156486146097,"d":"0.20"}]
["01079","01","AL","079","Lawrence","","2104009000","Wax Log; Total: All Combustor Types",null,187.5229647383887,"A","CEC Survey",2017,15,"I",64.4007773763989,"TON",8,{"v":0.34342874999999995,"d":"0.34"},{"$f":"VLOOKUP(A598,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.2703311948992443,"d":"0.27"}]
["01079","01","AL","079","Lawrence","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",584.9574086630399,"A","CEC Survey",2017,15,"I",558.00332696756,"TON",8,{"v":0.9539212918815999,"d":"0.95"},{"$f":"VLOOKUP(A599,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.7508826289999999,"d":"0.75"}]
["01079","01","AL","079","Lawrence","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",773.65334694144,"A","CEC Survey",2017,15,"I",738.004400182902,"TON",8,{"v":0.9539212918815999,"d":"0.95"},{"$f":"VLOOKUP(A600,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.7508826289999999,"d":"0.75"}]
["01079","01","AL","079","Lawrence","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",528.34862717952,"A","CEC Survey",2017,15,"I",504.00300500295754,"TON",8,{"v":0.9539212918815999,"d":"0.95"},{"$f":"VLOOKUP(A601,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.7508826289999999,"d":"0.75"}]
["01081","01","AL","081","Lee","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",175.0727861227813,"A","CEC Survey",2017,15,"I",247.74042271644834,"TON",8,{"v":1.4150710010561212,"d":"1.42"},{"$f":"VLOOKUP(A602,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":1.1817863713513623,"d":"1.18"}]
["01081","01","AL","081","Lee","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.195090766711997,"A","CEC Survey",2017,15,"I",20.087061301333648,"TON",8,{"v":1.4150710010561212,"d":"1.42"},{"$f":"VLOOKUP(A603,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":1.1817863713513623,"d":"1.18"}]
["01081","01","AL","081","Lee","","2104008610","Hydronic heater: outdoor","Hydronic heater",170.34108920054396,"A","CEC Survey",2017,15,"I",241.04473561600378,"TON",8,{"v":1.4150710010561212,"d":"1.42"},{"$f":"VLOOKUP(A604,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":1.1817863713513623,"d":"1.18"}]
["01081","01","AL","081","Lee","","2104008620","Hydronic heater: indoor","Hydronic heater",108.82902921145865,"A","CEC Survey",2017,15,"I",154.00080331022465,"TON",8,{"v":1.4150710010561214,"d":"1.42"},{"$f":"VLOOKUP(A605,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":1.1817863713513623,"d":"1.18"}]
["01081","01","AL","081","Lee","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.731696922237332,"A","CEC Survey",2017,15,"I",6.69568710044455,"TON",8,{"v":1.4150710010561214,"d":"1.42"},{"$f":"VLOOKUP(A606,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":1.1817863713513623,"d":"1.18"}]
["01081","01","AL","081","Lee","","2104008100","Fireplace: general","Fireplace: general",5838.603316701,"A","CEC Survey",2017,15,"I",1149.4499884630882,"TON",8,{"v":0.1968707113866,"d":"0.20"},{"$f":"VLOOKUP(A607,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.164415159,"d":"0.16"}]
["01081","01","AL","081","Lee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1345.8795849717599,"A","CEC Survey",2017,15,"I",696.9783375589705,"TON",8,{"v":0.517860843824,"d":"0.52"},{"$f":"VLOOKUP(A608,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.43248776,"d":"0.43"}]
["01081","01","AL","081","Lee","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1780.0342898013598,"A","CEC Survey",2017,15,"I",921.8100593521867,"TON",8,{"v":0.517860843824,"d":"0.52"},{"$f":"VLOOKUP(A609,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.43248776,"d":"0.43"}]
["01081","01","AL","081","Lee","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1215.63317352288,"A","CEC Survey",2017,15,"I",629.5288210210057,"TON",8,{"v":0.517860843824,"d":"0.52"},{"$f":"VLOOKUP(A610,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.43248776,"d":"0.43"}]
["01081","01","AL","081","Lee","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,6954.39948918,"A","CEC Survey",2017,15,"I",1213.706238344535,"TON",8,{"v":0.1745235142492,"d":"0.17"},{"$f":"VLOOKUP(A611,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.14575205800000002,"d":"0.15"}]
["01081","01","AL","081","Lee","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1362.943396344,"A","CEC Survey",2017,15,"I",323.2087854478841,"TON",8,{"v":0.237140285,"d":"0.24"},{"$f":"VLOOKUP(A612,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.19804600384165694,"d":"0.20"}]
["01081","01","AL","081","Lee","","2104009000","Wax Log; Total: All Combustor Types",null,847.4297213947359,"A","CEC Survey",2017,15,"I",198.4106697585087,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A613,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.19553390679806243,"d":"0.20"}]
["01081","01","AL","081","Lee","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1496.1277507876803,"A","CEC Survey",2017,15,"I",1135.023155960044,"TON",8,{"v":0.7586405341138001,"d":"0.76"},{"$f":"VLOOKUP(A614,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.6335731870000001,"d":"0.63"}]
["01081","01","AL","081","Lee","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1978.7496058804802,"A","CEC Survey",2017,15,"I",1501.1596578826388,"TON",8,{"v":0.7586405341138001,"d":"0.76"},{"$f":"VLOOKUP(A615,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.6335731870000001,"d":"0.63"}]
["01081","01","AL","081","Lee","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1351.3411942598402,"A","CEC Survey",2017,15,"I",1025.1822053832657,"TON",8,{"v":0.7586405341138001,"d":"0.76"},{"$f":"VLOOKUP(A616,cordwood_density!A:D,4,FALSE)","v":1.1974},{"v":0.6335731870000001,"d":"0.63"}]
["01083","01","AL","083","Limestone","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",159.51340861499068,"A","CEC Survey",2017,15,"I",269.4537747908573,"TON",8,{"v":1.6892233520081315,"d":"1.69"},{"$f":"VLOOKUP(A617,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":1.2487789990449705,"d":"1.25"}]
["01083","01","AL","083","Limestone","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",12.933519617431678,"A","CEC Survey",2017,15,"I",21.847603361420862,"TON",8,{"v":1.6892233520081312,"d":"1.69"},{"$f":"VLOOKUP(A618,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":1.2487789990449703,"d":"1.25"}]
["01083","01","AL","083","Limestone","","2104008610","Hydronic heater: outdoor","Hydronic heater",155.20223540918013,"A","CEC Survey",2017,15,"I",262.17124033705034,"TON",8,{"v":1.6892233520081312,"d":"1.69"},{"$f":"VLOOKUP(A619,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":1.2487789990449703,"d":"1.25"}]
["01083","01","AL","083","Limestone","","2104008620","Hydronic heater: indoor","Hydronic heater",99.15698373364287,"A","CEC Survey",2017,15,"I",167.49829243755997,"TON",8,{"v":1.6892233520081312,"d":"1.69"},{"$f":"VLOOKUP(A620,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":1.2487789990449703,"d":"1.25"}]
["01083","01","AL","083","Limestone","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.31117320581056,"A","CEC Survey",2017,15,"I",7.282534453806955,"TON",8,{"v":1.6892233520081312,"d":"1.69"},{"$f":"VLOOKUP(A621,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":1.2487789990449703,"d":"1.25"}]
["01083","01","AL","083","Limestone","","2104008100","Fireplace: general","Fireplace: general",2090.133788954,"A","CEC Survey",2017,15,"I",584.1223740391135,"TON",8,{"v":0.2794664997648,"d":"0.28"},{"$f":"VLOOKUP(A622,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.206599024,"d":"0.21"}]
["01083","01","AL","083","Limestone","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",783.96930981942,"A","CEC Survey",2017,15,"I",300.2658037751094,"TON",8,{"v":0.383007089709,"d":"0.38"},{"$f":"VLOOKUP(A623,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.28314267,"d":"0.28"}]
["01083","01","AL","083","Limestone","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1036.86263556762,"A","CEC Survey",2017,15,"I",397.1257404767576,"TON",8,{"v":0.383007089709,"d":"0.38"},{"$f":"VLOOKUP(A624,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.28314267,"d":"0.28"}]
["01083","01","AL","083","Limestone","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",708.1013120949601,"A","CEC Survey",2017,15,"I",271.207822764615,"TON",8,{"v":0.383007089709,"d":"0.38"},{"$f":"VLOOKUP(A625,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.28314267,"d":"0.28"}]
["01083","01","AL","083","Limestone","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4877.160407603999,"A","CEC Survey",2017,15,"I",976.8100981185358,"TON",8,{"v":0.2002825448586,"d":"0.20"},{"$f":"VLOOKUP(A626,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.148061318,"d":"0.15"}]
["01083","01","AL","083","Limestone","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1216.7031568,"A","CEC Survey",2017,15,"I",251.64997416542465,"TON",8,{"v":0.206829392,"d":"0.21"},{"$f":"VLOOKUP(A627,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.15290115472758187,"d":"0.15"}]
["01083","01","AL","083","Limestone","","2104009000","Wax Log; Total: All Combustor Types",null,465.1592169131018,"A","CEC Survey",2017,15,"I",159.7490484154454,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A628,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.2538838988689288,"d":"0.25"}]
["01083","01","AL","083","Limestone","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1241.86893581324,"A","CEC Survey",2017,15,"I",1104.9403975077691,"TON",8,{"v":0.8897399440821,"d":"0.89"},{"$f":"VLOOKUP(A629,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.6577511229999999,"d":"0.66"}]
["01083","01","AL","083","Limestone","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1642.47181833364,"A","CEC Survey",2017,15,"I",1461.372783800598,"TON",8,{"v":0.8897399440821,"d":"0.89"},{"$f":"VLOOKUP(A630,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.6577511229999999,"d":"0.66"}]
["01083","01","AL","083","Limestone","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1121.6880710571202,"A","CEC Survey",2017,15,"I",998.0106816199207,"TON",8,{"v":0.8897399440821,"d":"0.89"},{"$f":"VLOOKUP(A631,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.6577511229999999,"d":"0.66"}]
["01085","01","AL","085","Lowndes","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",22.545628171073712,"A","CEC Survey",2017,15,"I",35.85370451333362,"TON",8,{"v":1.5902730339239033,"d":"1.59"},{"$f":"VLOOKUP(A632,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":1.2410434165162347,"d":"1.24"}]
["01085","01","AL","085","Lowndes","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.8280239057627334,"A","CEC Survey",2017,15,"I",2.9070571227027258,"TON",8,{"v":1.5902730339239033,"d":"1.59"},{"$f":"VLOOKUP(A633,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":1.2410434165162347,"d":"1.24"}]
["01085","01","AL","085","Lowndes","","2104008610","Hydronic heater: outdoor","Hydronic heater",21.936286869152802,"A","CEC Survey",2017,15,"I",34.88468547243271,"TON",8,{"v":1.5902730339239033,"d":"1.59"},{"$f":"VLOOKUP(A634,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":1.2410434165162347,"d":"1.24"}]
["01085","01","AL","085","Lowndes","","2104008620","Hydronic heater: indoor","Hydronic heater",14.014849944180957,"A","CEC Survey",2017,15,"I",22.2874379407209,"TON",8,{"v":1.5902730339239033,"d":"1.59"},{"$f":"VLOOKUP(A635,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":1.2410434165162347,"d":"1.24"}]
["01085","01","AL","085","Lowndes","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.6093413019209112,"A","CEC Survey",2017,15,"I",0.9690190409009087,"TON",8,{"v":1.5902730339239035,"d":"1.59"},{"$f":"VLOOKUP(A636,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":1.241043416516235,"d":"1.24"}]
["01085","01","AL","085","Lowndes","","2104008100","Fireplace: general","Fireplace: general",310.95728294500003,"A","CEC Survey",2017,15,"I",90.67181285057306,"TON",8,{"v":0.2915892883802,"d":"0.29"},{"$f":"VLOOKUP(A637,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.22755524299999996,"d":"0.23"}]
["01085","01","AL","085","Lowndes","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",126.09097802647999,"A","CEC Survey",2017,15,"I",62.06857665928826,"TON",8,{"v":0.49225232154399995,"d":"0.49"},{"$f":"VLOOKUP(A638,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.38415195999999996,"d":"0.38"}]
["01085","01","AL","085","Lowndes","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",166.76548706727996,"A","CEC Survey",2017,15,"I",82.09069816228447,"TON",8,{"v":0.492252321544,"d":"0.49"},{"$f":"VLOOKUP(A639,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.38415195999999996,"d":"0.38"}]
["01085","01","AL","085","Lowndes","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",113.88862531424,"A","CEC Survey",2017,15,"I",56.0619402083894,"TON",8,{"v":0.49225232154399995,"d":"0.49"},{"$f":"VLOOKUP(A640,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.38415195999999996,"d":"0.38"}]
["01085","01","AL","085","Lowndes","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,588.390800121,"A","CEC Survey",2017,15,"I",109.56137048303225,"TON",8,{"v":0.18620510460140002,"d":"0.19"},{"$f":"VLOOKUP(A641,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.14531380100000002,"d":"0.15"}]
["01085","01","AL","085","Lowndes","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",145.336683906,"A","CEC Survey",2017,15,"I",37.67431676004344,"TON",8,{"v":0.259220974,"d":"0.26"},{"$f":"VLOOKUP(A642,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.20229512564382704,"d":"0.20"}]
["01085","01","AL","085","Lowndes","","2104009000","Wax Log; Total: All Combustor Types",null,61.89004710920014,"A","CEC Survey",2017,15,"I",14.49045907678538,"TON",8,{"$f":"P643/J643","v":{"v":0.2341323,"d":"0.23"}},{"$f":"VLOOKUP(A643,cordwood_density!A:D,4,FALSE)","v":1.2814},{"$f":"S643/T643","v":{"v":0.18271601373497734,"d":"0.18"}}]
["01085","01","AL","085","Lowndes","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",181.57749858772,"A","CEC Survey",2017,15,"I",184.5037309521446,"TON",8,{"v":1.0161156111698,"d":"1.02"},{"$f":"VLOOKUP(A644,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.792973007,"d":"0.79"}]
["01085","01","AL","085","Lowndes","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",240.15088522891998,"A","CEC Survey",2017,15,"I",244.02106351735253,"TON",8,{"v":1.0161156111698,"d":"1.02"},{"$f":"VLOOKUP(A645,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.792973007,"d":"0.79"}]
["01085","01","AL","085","Lowndes","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",164.00548259536,"A","CEC Survey",2017,15,"I",166.64853118258225,"TON",8,{"v":1.0161156111698002,"d":"1.02"},{"$f":"VLOOKUP(A646,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":0.7929730070000001,"d":"0.79"}]
["01087","01","AL","087","Macon","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",31.7805139614578,"A","CEC Survey",2017,15,"I",49.96630743913981,"TON",8,{"v":1.5722309431413555,"d":"1.57"},{"$f":"VLOOKUP(A647,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":1.1608320607954485,"d":"1.16"}]
["01087","01","AL","087","Macon","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.5767984293073893,"A","CEC Survey",2017,15,"I",4.051322224795119,"TON",8,{"v":1.572230943141355,"d":"1.57"},{"$f":"VLOOKUP(A648,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":1.160832060795448,"d":"1.16"}]
["01087","01","AL","087","Macon","","2104008610","Hydronic heater: outdoor","Hydronic heater",30.92158115168867,"A","CEC Survey",2017,15,"I",48.615866697541435,"TON",8,{"v":1.5722309431413553,"d":"1.57"},{"$f":"VLOOKUP(A649,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":1.1608320607954483,"d":"1.16"}]
["01087","01","AL","087","Macon","","2104008620","Hydronic heater: indoor","Hydronic heater",19.755454624689985,"A","CEC Survey",2017,15,"I",31.060137056762585,"TON",8,{"v":1.5722309431413553,"d":"1.57"},{"$f":"VLOOKUP(A650,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":1.1608320607954483,"d":"1.16"}]
["01087","01","AL","087","Macon","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8589328097691298,"A","CEC Survey",2017,15,"I",1.3504407415983732,"TON",8,{"v":1.5722309431413553,"d":"1.57"},{"$f":"VLOOKUP(A651,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":1.1608320607954483,"d":"1.16"}]
["01087","01","AL","087","Macon","","2104008100","Fireplace: general","Fireplace: general",966.0642321720001,"A","CEC Survey",2017,15,"I",262.99140773153835,"TON",8,{"v":0.27222973273760004,"d":"0.27"},{"$f":"VLOOKUP(A652,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.20099655400000002,"d":"0.20"}]
["01087","01","AL","087","Macon","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",194.037762243,"A","CEC Survey",2017,15,"I",116.74300222611514,"TON",8,{"v":0.6016509409128,"d":"0.60"},{"$f":"VLOOKUP(A653,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.444219537,"d":"0.44"}]
["01087","01","AL","087","Macon","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",256.630588773,"A","CEC Survey",2017,15,"I",154.4020352022813,"TON",8,{"v":0.6016509409128,"d":"0.60"},{"$f":"VLOOKUP(A654,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.444219537,"d":"0.44"}]
["01087","01","AL","087","Macon","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",175.25991428400002,"A","CEC Survey",2017,15,"I",105.4452923332653,"TON",8,{"v":0.6016509409128,"d":"0.60"},{"$f":"VLOOKUP(A655,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.444219537,"d":"0.44"}]
["01087","01","AL","087","Macon","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1109.8832936879999,"A","CEC Survey",2017,15,"I",220.72922991321875,"TON",8,{"v":0.1988760720776,"d":"0.20"},{"$f":"VLOOKUP(A656,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.14683702899999998,"d":"0.15"}]
["01087","01","AL","087","Macon","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",249.75536383199997,"A","CEC Survey",2017,15,"I",51.4949507830047,"TON",8,{"v":0.206181561,"d":"0.21"},{"$f":"VLOOKUP(A657,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.1522309221795629,"d":"0.15"}]
["01087","01","AL","087","Macon","","2104009000","Wax Log; Total: All Combustor Types",null,112.77805753108366,"A","CEC Survey",2017,15,"I",26.40498599928494,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A658,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.1728679119905493,"d":"0.17"}]
["01087","01","AL","087","Macon","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",236.84841489296002,"A","CEC Survey",2017,15,"I",227.98845783840449,"TON",8,{"v":0.9625922890023999,"d":"0.96"},{"$f":"VLOOKUP(A659,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.7107149209999999,"d":"0.71"}]
["01087","01","AL","087","Macon","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",313.25112937456,"A","CEC Survey",2017,15,"I",301.53312165724464,"TON",8,{"v":0.9625922890024,"d":"0.96"},{"$f":"VLOOKUP(A660,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.710714921,"d":"0.71"}]
["01087","01","AL","087","Macon","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",213.92760054848003,"A","CEC Survey",2017,15,"I",205.92505869275246,"TON",8,{"v":0.9625922890023999,"d":"0.96"},{"$f":"VLOOKUP(A661,cordwood_density!A:D,4,FALSE)","v":1.3544},{"v":0.7107149209999999,"d":"0.71"}]
["01089","01","AL","089","Madison","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",406.8012259489687,"A","CEC Survey",2017,15,"I",570.1474006803822,"TON",8,{"v":1.4015380591598918,"d":"1.40"},{"$f":"VLOOKUP(A662,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":1.183631500008354,"d":"1.18"}]
["01089","01","AL","089","Madison","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",32.98388318505152,"A","CEC Survey",2017,15,"I",46.22816762273369,"TON",8,{"v":1.4015380591598918,"d":"1.40"},{"$f":"VLOOKUP(A663,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":1.183631500008354,"d":"1.18"}]
["01089","01","AL","089","Madison","","2104008610","Hydronic heater: outdoor","Hydronic heater",395.8065982206182,"A","CEC Survey",2017,15,"I",554.7380114728044,"TON",8,{"v":1.401538059159892,"d":"1.40"},{"$f":"VLOOKUP(A664,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":1.1836315000083542,"d":"1.18"}]
["01089","01","AL","089","Madison","","2104008620","Hydronic heater: indoor","Hydronic heater",252.87643775206166,"A","CEC Survey",2017,15,"I",354.41595177429167,"TON",8,{"v":1.4015380591598916,"d":"1.40"},{"$f":"VLOOKUP(A665,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":1.1836315000083537,"d":"1.18"}]
["01089","01","AL","089","Madison","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.994627728350507,"A","CEC Survey",2017,15,"I",15.409389207577899,"TON",8,{"v":1.4015380591598918,"d":"1.40"},{"$f":"VLOOKUP(A666,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":1.183631500008354,"d":"1.18"}]
["01089","01","AL","089","Madison","","2104008100","Fireplace: general","Fireplace: general",12387.735350006998,"A","CEC Survey",2017,15,"I",2381.025898842024,"TON",8,{"v":0.19220832796049997,"d":"0.19"},{"$f":"VLOOKUP(A667,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.16232440499999998,"d":"0.16"}]
["01089","01","AL","089","Madison","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",2886.74417183026,"A","CEC Survey",2017,15,"I",1129.4658384883955,"TON",8,{"v":0.39125941588799995,"d":"0.39"},{"$f":"VLOOKUP(A668,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.33042768,"d":"0.33"}]
["01089","01","AL","089","Madison","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3817.9519691948594,"A","CEC Survey",2017,15,"I",1493.80965735562,"TON",8,{"v":0.39125941588799995,"d":"0.39"},{"$f":"VLOOKUP(A669,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.33042768,"d":"0.33"}]
["01089","01","AL","089","Madison","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",2607.38183262088,"A","CEC Survey",2017,15,"I",1020.1626928282284,"TON",8,{"v":0.391259415888,"d":"0.39"},{"$f":"VLOOKUP(A670,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.33042768,"d":"0.33"}]
["01089","01","AL","089","Madison","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,18031.772206151003,"A","CEC Survey",2017,15,"I",3246.779565109147,"TON",8,{"v":0.180058816626,"d":"0.18"},{"$f":"VLOOKUP(A671,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.15206386000000002,"d":"0.15"}]
["01089","01","AL","089","Madison","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",3768.145691626,"A","CEC Survey",2017,15,"I",753.7792197999518,"TON",8,{"v":0.200039829,"d":"0.20"},{"$f":"VLOOKUP(A672,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.16893828984038511,"d":"0.17"}]
["01089","01","AL","089","Madison","","2104009000","Wax Log; Total: All Combustor Types",null,2043.1758810454971,"A","CEC Survey",2017,15,"I",701.6853388576038,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A673,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.290033569799848,"d":"0.29"}]
["01089","01","AL","089","Madison","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",3573.93031520927,"A","CEC Survey",2017,15,"I",2336.262769390111,"TON",8,{"v":0.6536956692881999,"d":"0.65"},{"$f":"VLOOKUP(A674,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.552061202,"d":"0.55"}]
["01089","01","AL","089","Madison","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",4726.811062050969,"A","CEC Survey",2017,15,"I",3089.895920806275,"TON",8,{"v":0.6536956692881999,"d":"0.65"},{"$f":"VLOOKUP(A675,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.552061202,"d":"0.55"}]
["01089","01","AL","089","Madison","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",3228.0660911567597,"A","CEC Survey",2017,15,"I",2110.1728239652616,"TON",8,{"v":0.6536956692882,"d":"0.65"},{"$f":"VLOOKUP(A676,cordwood_density!A:D,4,FALSE)","v":1.1841},{"v":0.5520612020000001,"d":"0.55"}]
["01091","01","AL","091","Marengo","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",38.333018837971636,"A","CEC Survey",2017,15,"I",57.36785516896593,"TON",8,{"v":1.496565021697141,"d":"1.50"},{"$f":"VLOOKUP(A677,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":1.207296726119023,"d":"1.21"}]
["01091","01","AL","091","Marengo","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.108082608484187,"A","CEC Survey",2017,15,"I",4.651447716402643,"TON",8,{"v":1.4965650216971407,"d":"1.50"},{"$f":"VLOOKUP(A678,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":1.2072967261190228,"d":"1.21"}]
["01091","01","AL","091","Marengo","","2104008610","Hydronic heater: outdoor","Hydronic heater",37.296991301810245,"A","CEC Survey",2017,15,"I",55.81737259683172,"TON",8,{"v":1.4965650216971407,"d":"1.50"},{"$f":"VLOOKUP(A679,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":1.2072967261190228,"d":"1.21"}]
["01091","01","AL","091","Marengo","","2104008620","Hydronic heater: indoor","Hydronic heater",23.8286333317121,"A","CEC Survey",2017,15,"I",35.66109915908693,"TON",8,{"v":1.4965650216971407,"d":"1.50"},{"$f":"VLOOKUP(A680,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":1.2072967261190228,"d":"1.21"}]
["01091","01","AL","091","Marengo","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0360275361613958,"A","CEC Survey",2017,15,"I",1.5504825721342144,"TON",8,{"v":1.4965650216971407,"d":"1.50"},{"$f":"VLOOKUP(A681,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":1.2072967261190228,"d":"1.21"}]
["01091","01","AL","091","Marengo","","2104008100","Fireplace: general","Fireplace: general",899.27639175,"A","CEC Survey",2017,15,"I",227.32022718507017,"TON",8,{"v":0.25278126866280004,"d":"0.25"},{"$f":"VLOOKUP(A682,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.203921643,"d":"0.20"}]
["01091","01","AL","091","Marengo","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",230.74031141975,"A","CEC Survey",2017,15,"I",129.13170508238713,"TON",8,{"v":0.5596408546379998,"d":"0.56"},{"$f":"VLOOKUP(A683,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.45146890499999986,"d":"0.45"}]
["01091","01","AL","091","Marengo","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",305.17266994224997,"A","CEC Survey",2017,15,"I",170.78709381864104,"TON",8,{"v":0.559640854638,"d":"0.56"},{"$f":"VLOOKUP(A684,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.4514689049999999,"d":"0.45"}]
["01091","01","AL","091","Marengo","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",208.410603863,"A","CEC Survey",2017,15,"I",116.63508846151097,"TON",8,{"v":0.559640854638,"d":"0.56"},{"$f":"VLOOKUP(A685,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.4514689049999999,"d":"0.45"}]
["01091","01","AL","091","Marengo","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1184.9905122,"A","CEC Survey",2017,15,"I",216.76829705752215,"TON",8,{"v":0.18292829759040002,"d":"0.18"},{"$f":"VLOOKUP(A686,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.147570424,"d":"0.15"}]
["01091","01","AL","091","Marengo","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",276.34410155,"A","CEC Survey",2017,15,"I",65.53157756841148,"TON",8,{"v":0.23713760199999998,"d":"0.24"},{"$f":"VLOOKUP(A687,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.1913017118425298,"d":"0.19"}]
["01091","01","AL","091","Marengo","","2104009000","Wax Log; Total: All Combustor Types",null,114.54470310881204,"A","CEC Survey",2017,15,"I",26.818614791683313,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A688,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.1888772991287512,"d":"0.19"}]
["01091","01","AL","091","Marengo","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",291.383884495,"A","CEC Survey",2017,15,"I",265.9179308062766,"TON",8,{"v":0.912603424404,"d":"0.91"},{"$f":"VLOOKUP(A689,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.7362079899999999,"d":"0.74"}]
["01091","01","AL","091","Marengo","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",385.378685945,"A","CEC Survey",2017,15,"I",351.6979084857207,"TON",8,{"v":0.9126034244040001,"d":"0.91"},{"$f":"VLOOKUP(A690,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.73620799,"d":"0.74"}]
["01091","01","AL","091","Marengo","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",263.18544406,"A","CEC Survey",2017,15,"I",240.18393750244343,"TON",8,{"v":0.9126034244040001,"d":"0.91"},{"$f":"VLOOKUP(A691,cordwood_density!A:D,4,FALSE)","v":1.2396},{"v":0.73620799,"d":"0.74"}]
["01093","01","AL","093","Marion","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",77.88273823655908,"A","CEC Survey",2017,15,"I",118.83444903997682,"TON",8,{"v":1.5258124165977838,"d":"1.53"},{"$f":"VLOOKUP(A692,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":1.1656320982412405,"d":"1.17"}]
["01093","01","AL","093","Marion","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.3148166137750605,"A","CEC Survey",2017,15,"I",9.635225597835957,"TON",8,{"v":1.5258124165977835,"d":"1.53"},{"$f":"VLOOKUP(A693,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":1.1656320982412403,"d":"1.17"}]
["01093","01","AL","093","Marion","","2104008610","Hydronic heater: outdoor","Hydronic heater",75.77779936530072,"A","CEC Survey",2017,15,"I",115.62270717403149,"TON",8,{"v":1.5258124165977835,"d":"1.53"},{"$f":"VLOOKUP(A694,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":1.1656320982412403,"d":"1.17"}]
["01093","01","AL","093","Marion","","2104008620","Hydronic heater: indoor","Hydronic heater",48.413594038942136,"A","CEC Survey",2017,15,"I",73.87006291674234,"TON",8,{"v":1.5258124165977833,"d":"1.53"},{"$f":"VLOOKUP(A695,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":1.1656320982412403,"d":"1.17"}]
["01093","01","AL","093","Marion","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.1049388712583537,"A","CEC Survey",2017,15,"I",3.2117418659453194,"TON",8,{"v":1.5258124165977835,"d":"1.53"},{"$f":"VLOOKUP(A696,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":1.1656320982412403,"d":"1.17"}]
["01093","01","AL","093","Marion","","2104008100","Fireplace: general","Fireplace: general",1756.096618521,"A","CEC Survey",2017,15,"I",490.62398950684144,"TON",8,{"v":0.279383255074,"d":"0.28"},{"$f":"VLOOKUP(A697,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.21343258600000004,"d":"0.21"}]
["01093","01","AL","093","Marion","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",304.41116177072996,"A","CEC Survey",2017,15,"I",182.00771686908635,"TON",8,{"v":0.597900930473,"d":"0.60"},{"$f":"VLOOKUP(A698,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.456761597,"d":"0.46"}]
["01093","01","AL","093","Marion","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",402.60831072902994,"A","CEC Survey",2017,15,"I",240.71988360104967,"TON",8,{"v":0.5979009304729999,"d":"0.60"},{"$f":"VLOOKUP(A699,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.4567615969999999,"d":"0.46"}]
["01093","01","AL","093","Marion","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",274.95201708324,"A","CEC Survey",2017,15,"I",164.39406684949736,"TON",8,{"v":0.597900930473,"d":"0.60"},{"$f":"VLOOKUP(A700,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.456761597,"d":"0.46"}]
["01093","01","AL","093","Marion","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1943.810861622,"A","CEC Survey",2017,15,"I",373.0101942272406,"TON",8,{"v":0.19189634217599996,"d":"0.19"},{"$f":"VLOOKUP(A701,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.146597664,"d":"0.15"}]
["01093","01","AL","093","Marion","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",484.637983704,"A","CEC Survey",2017,15,"I",121.93713488797782,"TON",8,{"v":0.251604577,"d":"0.25"},{"$f":"VLOOKUP(A702,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.19221128877005347,"d":"0.19"}]
["01093","01","AL","093","Marion","","2104009000","Wax Log; Total: All Combustor Types",null,178.86209251586664,"A","CEC Survey",2017,15,"I",61.42638485510844,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A703,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.2623596256684492,"d":"0.26"}]
["01093","01","AL","093","Marion","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",450.44720224224005,"A","CEC Survey",2017,15,"I",458.13273488345584,"TON",8,{"v":1.017062005498,"d":"1.02"},{"$f":"VLOOKUP(A704,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.776976322,"d":"0.78"}]
["01093","01","AL","093","Marion","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",595.75275135264,"A","CEC Survey",2017,15,"I",605.9174880716673,"TON",8,{"v":1.017062005498,"d":"1.02"},{"$f":"VLOOKUP(A705,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.776976322,"d":"0.78"}]
["01093","01","AL","093","Marion","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",406.8555375091201,"A","CEC Survey",2017,15,"I",413.7973089269924,"TON",8,{"v":1.017062005498,"d":"1.02"},{"$f":"VLOOKUP(A706,cordwood_density!A:D,4,FALSE)","v":1.309},{"v":0.776976322,"d":"0.78"}]
["01095","01","AL","095","Marshall","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",160.2378725399351,"A","CEC Survey",2017,15,"I",275.53092376328175,"TON",8,{"$f":"P707/J707","v":{"v":1.7195118694215867,"d":"1.72"}},{"$f":"VLOOKUP(A707,cordwood_density!A:D,4,FALSE)","v":1.4183},{"$f":"S707/T707","v":{"v":1.2123752869079791,"d":"1.21"}}]
["01095","01","AL","095","Marshall","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",12.992259935670413,"A","CEC Survey",2017,15,"I",22.340345169995818,"TON",8,{"v":1.719511869421587,"d":"1.72"},{"$f":"VLOOKUP(A708,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":1.2123752869079794,"d":"1.21"}]
["01095","01","AL","095","Marshall","","2104008610","Hydronic heater: outdoor","Hydronic heater",155.90711922804493,"A","CEC Survey",2017,15,"I",268.0841420399498,"TON",8,{"v":1.7195118694215872,"d":"1.72"},{"$f":"VLOOKUP(A709,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":1.2123752869079796,"d":"1.21"}]
["01095","01","AL","095","Marshall","","2104008620","Hydronic heater: indoor","Hydronic heater",99.60732617347317,"A","CEC Survey",2017,15,"I",171.27597963663462,"TON",8,{"v":1.719511869421587,"d":"1.72"},{"$f":"VLOOKUP(A710,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":1.2123752869079794,"d":"1.21"}]
["01095","01","AL","095","Marshall","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.330753311890137,"A","CEC Survey",2017,15,"I",7.44678172333194,"TON",8,{"v":1.7195118694215872,"d":"1.72"},{"$f":"VLOOKUP(A711,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":1.2123752869079796,"d":"1.21"}]
["01095","01","AL","095","Marshall","","2104008100","Fireplace: general","Fireplace: general",3167.9140197961,"A","CEC Survey",2017,15,"I",892.0786259889076,"TON",8,{"v":0.2815981180089999,"d":"0.28"},{"$f":"VLOOKUP(A712,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.19854622999999996,"d":"0.20"}]
["01095","01","AL","095","Marshall","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",808.2038422753741,"A","CEC Survey",2017,15,"I",379.1625256142775,"TON",8,{"v":0.46914219628899995,"d":"0.47"},{"$f":"VLOOKUP(A713,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.33077783,"d":"0.33"}]
["01095","01","AL","095","Marshall","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1068.9147591383978,"A","CEC Survey",2017,15,"I",501.4730177479154,"TON",8,{"v":0.469142196289,"d":"0.47"},{"$f":"VLOOKUP(A714,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.33077783000000005,"d":"0.33"}]
["01095","01","AL","095","Marshall","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",729.990567216467,"A","CEC Survey",2017,15,"I",342.46937797418616,"TON",8,{"v":0.46914219628899995,"d":"0.47"},{"$f":"VLOOKUP(A715,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.33077783,"d":"0.33"}]
["01095","01","AL","095","Marshall","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5192.76768977868,"A","CEC Survey",2017,15,"I",1088.662677851407,"TON",8,{"v":0.20964979426949998,"d":"0.21"},{"$f":"VLOOKUP(A716,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.147817665,"d":"0.15"}]
["01095","01","AL","095","Marshall","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1232.1890601717523,"A","CEC Survey",2017,15,"I",258.2385741490386,"TON",8,{"v":0.20957707099999998,"d":"0.21"},{"$f":"VLOOKUP(A717,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.14776639004441938,"d":"0.15"}]
["01095","01","AL","095","Marshall","","2104009000","Wax Log; Total: All Combustor Types",null,496.7864815024631,"A","CEC Survey",2017,15,"I",170.61076035928903,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A718,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.24214111965028556,"d":"0.24"}]
["01095","01","AL","095","Marshall","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1176.2071491257375,"A","CEC Survey",2017,15,"I",1116.5087862348082,"TON",8,{"v":0.9492450263244,"d":"0.95"},{"$f":"VLOOKUP(A719,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.669283668,"d":"0.67"}]
["01095","01","AL","095","Marshall","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1555.62881013404,"A","CEC Survey",2017,15,"I",1476.6729108266818,"TON",8,{"v":0.9492450263244,"d":"0.95"},{"$f":"VLOOKUP(A720,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.669283668,"d":"0.67"}]
["01095","01","AL","095","Marshall","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1062.380650823247,"A","CEC Survey",2017,15,"I",1008.4595488572463,"TON",8,{"v":0.9492450263244001,"d":"0.95"},{"$f":"VLOOKUP(A721,cordwood_density!A:D,4,FALSE)","v":1.4183},{"v":0.6692836680000002,"d":"0.67"}]
["01097","01","AL","097","Mobile","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",289.0041247033883,"A","CEC Survey",2017,15,"I",376.83144965864085,"TON",8,{"v":1.3038964410815652,"d":"1.30"},{"$f":"VLOOKUP(A722,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":1.0633635957279117,"d":"1.06"}]
["01097","01","AL","097","Mobile","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",23.432766867842297,"A","CEC Survey",2017,15,"I",30.553901323673582,"TON",8,{"v":1.303896441081565,"d":"1.30"},{"$f":"VLOOKUP(A723,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":1.0633635957279115,"d":"1.06"}]
["01097","01","AL","097","Mobile","","2104008610","Hydronic heater: outdoor","Hydronic heater",281.19320241410753,"A","CEC Survey",2017,15,"I",366.646815884083,"TON",8,{"v":1.3038964410815652,"d":"1.30"},{"$f":"VLOOKUP(A724,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":1.0633635957279117,"d":"1.06"}]
["01097","01","AL","097","Mobile","","2104008620","Hydronic heater: indoor","Hydronic heater",179.6512126534576,"A","CEC Survey",2017,15,"I",234.24657681483083,"TON",8,{"v":1.3038964410815652,"d":"1.30"},{"$f":"VLOOKUP(A725,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":1.0633635957279117,"d":"1.06"}]
["01097","01","AL","097","Mobile","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",7.810922289280766,"A","CEC Survey",2017,15,"I",10.184633774557861,"TON",8,{"v":1.303896441081565,"d":"1.30"},{"$f":"VLOOKUP(A726,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":1.0633635957279115,"d":"1.06"}]
["01097","01","AL","097","Mobile","","2104008100","Fireplace: general","Fireplace: general",17631.571024344,"A","CEC Survey",2017,15,"I",3741.150776008126,"TON",8,{"v":0.21218476622659999,"d":"0.21"},{"$f":"VLOOKUP(A727,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.173042543,"d":"0.17"}]
["01097","01","AL","097","Mobile","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",3062.58846274374,"A","CEC Survey",2017,15,"I",1344.6973719394407,"TON",8,{"v":0.4390721731952,"d":"0.44"},{"$f":"VLOOKUP(A728,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.358075496,"d":"0.36"}]
["01097","01","AL","097","Mobile","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",4050.5202249191398,"A","CEC Survey",2017,15,"I",1778.470717726357,"TON",8,{"v":0.4390721731952,"d":"0.44"},{"$f":"VLOOKUP(A729,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.358075496,"d":"0.36"}]
["01097","01","AL","097","Mobile","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",2766.20893409112,"A","CEC Survey",2017,15,"I",1214.5653682033658,"TON",8,{"v":0.4390721731951999,"d":"0.44"},{"$f":"VLOOKUP(A730,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.35807549599999994,"d":"0.36"}]
["01097","01","AL","097","Mobile","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,20664.368403536002,"A","CEC Survey",2017,15,"I",3790.522635851399,"TON",8,{"v":0.18343278448339997,"d":"0.18"},{"$f":"VLOOKUP(A731,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.149594507,"d":"0.15"}]
["01097","01","AL","097","Mobile","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",4171.30544792,"A","CEC Survey",2017,15,"I",497.70267576207124,"TON",8,{"v":0.119315807,"d":"0.12"},{"$f":"VLOOKUP(A732,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.0973053392595009,"d":"0.10"}]
["01097","01","AL","097","Mobile","","2104009000","Wax Log; Total: All Combustor Types",null,2208.938942936256,"A","CEC Survey",2017,15,"I",517.1839552692343,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A733,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.19094136356222474,"d":"0.19"}]
["01097","01","AL","097","Mobile","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",3041.3389210889,"A","CEC Survey",2017,15,"I",2032.9188422518798,"TON",8,{"v":0.6684289041762,"d":"0.67"},{"$f":"VLOOKUP(A734,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.545122251,"d":"0.55"}]
["01097","01","AL","097","Mobile","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",4022.4159924079,"A","CEC Survey",2017,15,"I",2688.6991139460347,"TON",8,{"v":0.6684289041762,"d":"0.67"},{"$f":"VLOOKUP(A735,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.545122251,"d":"0.55"}]
["01097","01","AL","097","Mobile","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2747.0157996932003,"A","CEC Survey",2017,15,"I",1836.1847607436337,"TON",8,{"v":0.6684289041762,"d":"0.67"},{"$f":"VLOOKUP(A736,cordwood_density!A:D,4,FALSE)","v":1.2262},{"v":0.545122251,"d":"0.55"}]
["01099","01","AL","099","Monroe","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",42.38768271359232,"A","CEC Survey",2017,15,"I",66.54091369413453,"TON",8,{"v":1.569817207129303,"d":"1.57"},{"$f":"VLOOKUP(A737,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":1.2000743116958206,"d":"1.20"}]
["01099","01","AL","099","Monroe","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.4368391389399178,"A","CEC Survey",2017,15,"I",5.39520921844334,"TON",8,{"v":1.569817207129303,"d":"1.57"},{"$f":"VLOOKUP(A738,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":1.2000743116958206,"d":"1.20"}]
["01099","01","AL","099","Monroe","","2104008610","Hydronic heater: outdoor","Hydronic heater",41.24206966727901,"A","CEC Survey",2017,15,"I",64.7425106213201,"TON",8,{"v":1.5698172071293033,"d":"1.57"},{"$f":"VLOOKUP(A739,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":1.2000743116958208,"d":"1.20"}]
["01099","01","AL","099","Monroe","","2104008620","Hydronic heater: indoor","Hydronic heater",26.349100065206038,"A","CEC Survey",2017,15,"I",41.363270674732284,"TON",8,{"v":1.5698172071293033,"d":"1.57"},{"$f":"VLOOKUP(A740,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":1.2000743116958208,"d":"1.20"}]
["01099","01","AL","099","Monroe","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.145613046313306,"A","CEC Survey",2017,15,"I",1.798403072814447,"TON",8,{"v":1.5698172071293028,"d":"1.57"},{"$f":"VLOOKUP(A741,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":1.2000743116958206,"d":"1.20"}]
["01099","01","AL","099","Monroe","","2104008100","Fireplace: general","Fireplace: general",867.5650640389999,"A","CEC Survey",2017,15,"I",237.90641200067859,"TON",8,{"v":0.2742231353728,"d":"0.27"},{"$f":"VLOOKUP(A742,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.209634688,"d":"0.21"}]
["01099","01","AL","099","Monroe","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",266.81996867935,"A","CEC Survey",2017,15,"I",163.52346097797098,"TON",8,{"v":0.6128606557723,"d":"0.61"},{"$f":"VLOOKUP(A743,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.46851208299999997,"d":"0.47"}]
["01099","01","AL","099","Monroe","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",352.89092631784996,"A","CEC Survey",2017,15,"I",216.27296451925196,"TON",8,{"v":0.6128606557723001,"d":"0.61"},{"$f":"VLOOKUP(A744,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.4685120830000001,"d":"0.47"}]
["01099","01","AL","099","Monroe","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",240.99868138780002,"A","CEC Survey",2017,15,"I",147.69860991558673,"TON",8,{"v":0.6128606557723001,"d":"0.61"},{"$f":"VLOOKUP(A745,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.4685120830000001,"d":"0.47"}]
["01099","01","AL","099","Monroe","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1279.471012755,"A","CEC Survey",2017,15,"I",246.6814634275487,"TON",8,{"v":0.19279957182960003,"d":"0.19"},{"$f":"VLOOKUP(A746,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.147389016,"d":"0.15"}]
["01099","01","AL","099","Monroe","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",307.13500098699996,"A","CEC Survey",2017,15,"I",75.43314865070973,"TON",8,{"v":0.24560257999999996,"d":"0.25"},{"$f":"VLOOKUP(A747,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.1877552022016665,"d":"0.19"}]
["01099","01","AL","099","Monroe","","2104009000","Wax Log; Total: All Combustor Types",null,117.87691265379567,"A","CEC Survey",2017,15,"I",27.598792676532284,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A748,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.17898654537114897,"d":"0.18"}]
["01099","01","AL","099","Monroe","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",335.28623949282996,"A","CEC Survey",2017,15,"I",326.6050259029446,"TON",8,{"v":0.9741080528595,"d":"0.97"},{"$f":"VLOOKUP(A749,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.744673995,"d":"0.74"}]
["01099","01","AL","099","Monroe","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",443.4430909421299,"A","CEC Survey",2017,15,"I",431.96148587163634,"TON",8,{"v":0.9741080528595,"d":"0.97"},{"$f":"VLOOKUP(A750,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.744673995,"d":"0.74"}]
["01099","01","AL","099","Monroe","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",302.83918405803996,"A","CEC Survey",2017,15,"I",294.99808791233704,"TON",8,{"v":0.9741080528595,"d":"0.97"},{"$f":"VLOOKUP(A751,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.744673995,"d":"0.74"}]
["01101","01","AL","101","Montgomery","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",175.535879425674,"A","CEC Survey",2017,15,"I",245.71856965427128,"TON",8,{"v":1.3998196292303549,"d":"1.40"},{"$f":"VLOOKUP(A752,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":1.0936945302213883,"d":"1.09"}]
["01101","01","AL","101","Montgomery","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.232638872351947,"A","CEC Survey",2017,15,"I",19.92312726926524,"TON",8,{"v":1.399819629230355,"d":"1.40"},{"$f":"VLOOKUP(A753,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":1.0936945302213885,"d":"1.09"}]
["01101","01","AL","101","Montgomery","","2104008610","Hydronic heater: outdoor","Hydronic heater",170.79166646822335,"A","CEC Survey",2017,15,"I",239.07752723118287,"TON",8,{"v":1.399819629230355,"d":"1.40"},{"$f":"VLOOKUP(A754,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":1.0936945302213885,"d":"1.09"}]
["01101","01","AL","101","Montgomery","","2104008620","Hydronic heater: indoor","Hydronic heater",109.11689802136493,"A","CEC Survey",2017,15,"I",152.74397573103352,"TON",8,{"v":1.399819629230355,"d":"1.40"},{"$f":"VLOOKUP(A755,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":1.0936945302213885,"d":"1.09"}]
["01101","01","AL","101","Montgomery","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.7442129574506495,"A","CEC Survey",2017,15,"I",6.641042423088414,"TON",8,{"v":1.3998196292303549,"d":"1.40"},{"$f":"VLOOKUP(A756,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":1.0936945302213883,"d":"1.09"}]
["01101","01","AL","101","Montgomery","","2104008100","Fireplace: general","Fireplace: general",12320.217149584001,"A","CEC Survey",2017,15,"I",2646.5233571996646,"TON",8,{"v":0.21481142134650005,"d":"0.21"},{"$f":"VLOOKUP(A757,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.16783453500000003,"d":"0.17"}]
["01101","01","AL","101","Montgomery","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1599.65374996752,"A","CEC Survey",2017,15,"I",799.7546981799338,"TON",8,{"v":0.4999548797333,"d":"0.50"},{"$f":"VLOOKUP(A758,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.39062026699999997,"d":"0.39"}]
["01101","01","AL","101","Montgomery","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2115.6710886667197,"A","CEC Survey",2017,15,"I",1057.7400846895898,"TON",8,{"v":0.49995487973330005,"d":"0.50"},{"$f":"VLOOKUP(A759,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.390620267,"d":"0.39"}]
["01101","01","AL","101","Montgomery","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1444.8485483577601,"A","CEC Survey",2017,15,"I",722.359082227037,"TON",8,{"v":0.49995487973329994,"d":"0.50"},{"$f":"VLOOKUP(A760,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.39062026699999997,"d":"0.39"}]
["01101","01","AL","101","Montgomery","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,11581.272240224,"A","CEC Survey",2017,15,"I",2207.9518724466775,"TON",8,{"v":0.1906484733843,"d":"0.19"},{"$f":"VLOOKUP(A761,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.148955757,"d":"0.15"}]
["01101","01","AL","101","Montgomery","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2226.662237472,"A","CEC Survey",2017,15,"I",293.8099860306435,"TON",8,{"v":0.131950855,"d":"0.13"},{"$f":"VLOOKUP(A762,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.10309465973904211,"d":"0.10"}]
["01101","01","AL","101","Montgomery","","2104009000","Wax Log; Total: All Combustor Types",null,1289.450190131249,"A","CEC Survey",2017,15,"I",301.90193875086663,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A763,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.1829301507930307,"d":"0.18"}]
["01101","01","AL","101","Montgomery","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1640.33039551344,"A","CEC Survey",2017,15,"I",1140.9272658480904,"TON",8,{"v":0.6955472318068999,"d":"0.70"},{"$f":"VLOOKUP(A764,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.543438731,"d":"0.54"}]
["01101","01","AL","101","Montgomery","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2169.46923277584,"A","CEC Survey",2017,15,"I",1508.9683193474746,"TON",8,{"v":0.6955472318069,"d":"0.70"},{"$f":"VLOOKUP(A765,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.5434387310000001,"d":"0.54"}]
["01101","01","AL","101","Montgomery","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1481.58874433472,"A","CEC Survey",2017,15,"I",1030.5149497982754,"TON",8,{"v":0.6955472318069,"d":"0.70"},{"$f":"VLOOKUP(A766,cordwood_density!A:D,4,FALSE)","v":1.2799},{"v":0.5434387310000001,"d":"0.54"}]
["01103","01","AL","103","Morgan","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",180.63353574220577,"A","CEC Survey",2017,15,"I",313.22274188446374,"TON",8,{"v":1.7340232011595285,"d":"1.73"},{"$f":"VLOOKUP(A767,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":1.236468340815408,"d":"1.24"}]
["01103","01","AL","103","Morgan","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.645962357476142,"A","CEC Survey",2017,15,"I",25.396438531172738,"TON",8,{"v":1.7340232011595287,"d":"1.73"},{"$f":"VLOOKUP(A768,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":1.2364683408154082,"d":"1.24"}]
["01103","01","AL","103","Morgan","","2104008610","Hydronic heater: outdoor","Hydronic heater",175.7515482897137,"A","CEC Survey",2017,15,"I",304.7572623740728,"TON",8,{"v":1.7340232011595285,"d":"1.73"},{"$f":"VLOOKUP(A769,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":1.236468340815408,"d":"1.24"}]
["01103","01","AL","103","Morgan","","2104008620","Hydronic heater: indoor","Hydronic heater",112.2857114073171,"A","CEC Survey",2017,15,"I",194.706028738991,"TON",8,{"v":1.7340232011595287,"d":"1.73"},{"$f":"VLOOKUP(A770,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":1.2364683408154082,"d":"1.24"}]
["01103","01","AL","103","Morgan","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.881987452492048,"A","CEC Survey",2017,15,"I",8.465479510390912,"TON",8,{"$f":"P771/J771","v":{"v":1.7340232011595285,"d":"1.73"}},{"$f":"VLOOKUP(A771,cordwood_density!A:D,4,FALSE)","v":1.4024},{"$f":"S771/T771","v":{"v":1.236468340815408,"d":"1.24"}}]
["01103","01","AL","103","Morgan","","2104008100","Fireplace: general","Fireplace: general",4033.9219653292266,"A","CEC Survey",2017,15,"I",1052.418689608009,"TON",8,{"v":0.2608921785432,"d":"0.26"},{"$f":"VLOOKUP(A772,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.186032643,"d":"0.19"}]
["01103","01","AL","103","Morgan","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1026.1579748356555,"A","CEC Survey",2017,15,"I",490.837806896229,"TON",8,{"v":0.47832577335360005,"d":"0.48"},{"$f":"VLOOKUP(A773,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.341076564,"d":"0.34"}]
["01103","01","AL","103","Morgan","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1357.1766763955443,"A","CEC Survey",2017,15,"I",649.1725833143673,"TON",8,{"v":0.47832577335360005,"d":"0.48"},{"$f":"VLOOKUP(A774,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.341076564,"d":"0.34"}]
["01103","01","AL","103","Morgan","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",926.8523643676889,"A","CEC Survey",2017,15,"I",443.3373739707875,"TON",8,{"v":0.47832577335360005,"d":"0.48"},{"$f":"VLOOKUP(A775,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.341076564,"d":"0.34"}]
["01103","01","AL","103","Morgan","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,6313.323368768668,"A","CEC Survey",2017,15,"I",1311.2850234444609,"TON",8,{"v":0.2077012291072,"d":"0.21"},{"$f":"VLOOKUP(A776,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.148104128,"d":"0.15"}]
["01103","01","AL","103","Morgan","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1402.113763710555,"A","CEC Survey",2017,15,"I",303.45546903028367,"TON",8,{"v":0.216427138,"d":"0.22"},{"$f":"VLOOKUP(A777,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.1543262535653166,"d":"0.15"}]
["01103","01","AL","103","Morgan","","2104009000","Wax Log; Total: All Combustor Types",null,659.3178746534746,"A","CEC Survey",2017,15,"I",226.42871354489947,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A778,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.24488644466628634,"d":"0.24"}]
["01103","01","AL","103","Morgan","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1407.8200555213118,"A","CEC Survey",2017,15,"I",1251.406182872289,"TON",8,{"v":0.8888964026080001,"d":"0.89"},{"$f":"VLOOKUP(A779,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.63383942,"d":"0.63"}]
["01103","01","AL","103","Morgan","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1861.9555573023802,"A","CEC Survey",2017,15,"I",1655.0855967020598,"TON",8,{"v":0.8888964026080002,"d":"0.89"},{"$f":"VLOOKUP(A780,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.63383942,"d":"0.63"}]
["01103","01","AL","103","Morgan","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1271.5794049869914,"A","CEC Survey",2017,15,"I",1130.302358723358,"TON",8,{"v":0.8888964026080002,"d":"0.89"},{"$f":"VLOOKUP(A781,cordwood_density!A:D,4,FALSE)","v":1.4024},{"v":0.63383942,"d":"0.63"}]
["01105","01","AL","105","Perry","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",17.904075274288797,"A","CEC Survey",2017,15,"I",27.195033178872983,"TON",8,{"v":1.5189297834290552,"d":"1.52"},{"$f":"VLOOKUP(A782,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":1.2021604934143688,"d":"1.20"}]
["01105","01","AL","105","Perry","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.451681778996389,"A","CEC Survey",2017,15,"I",2.2050026901788904,"TON",8,{"v":1.518929783429055,"d":"1.52"},{"$f":"VLOOKUP(A783,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":1.2021604934143686,"d":"1.20"}]
["01105","01","AL","105","Perry","","2104008610","Hydronic heater: outdoor","Hydronic heater",17.420181347956667,"A","CEC Survey",2017,15,"I",26.460032282146685,"TON",8,{"v":1.518929783429055,"d":"1.52"},{"$f":"VLOOKUP(A784,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":1.2021604934143686,"d":"1.20"}]
["01105","01","AL","105","Perry","","2104008620","Hydronic heater: indoor","Hydronic heater",11.129560305638982,"A","CEC Survey",2017,15,"I",16.90502062470483,"TON",8,{"v":1.5189297834290552,"d":"1.52"},{"$f":"VLOOKUP(A785,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":1.2021604934143688,"d":"1.20"}]
["01105","01","AL","105","Perry","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.48389392633212963,"A","CEC Survey",2017,15,"I",0.7350008967262969,"TON",8,{"v":1.5189297834290552,"d":"1.52"},{"$f":"VLOOKUP(A786,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":1.2021604934143688,"d":"1.20"}]
["01105","01","AL","105","Perry","","2104008100","Fireplace: general","Fireplace: general",337.056064371,"A","CEC Survey",2017,15,"I",95.60996046104373,"TON",8,{"v":0.28366189061,"d":"0.28"},{"$f":"VLOOKUP(A787,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.22450486,"d":"0.22"}]
["01105","01","AL","105","Perry","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",84.86792328570002,"A","CEC Survey",2017,15,"I",47.430366694943565,"TON",8,{"v":0.5588727149039999,"d":"0.56"},{"$f":"VLOOKUP(A788,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.4423211039999999,"d":"0.44"}]
["01105","01","AL","105","Perry","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",112.24467273270001,"A","CEC Survey",2017,15,"I",62.73048498363504,"TON",8,{"v":0.558872714904,"d":"0.56"},{"$f":"VLOOKUP(A789,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.442321104,"d":"0.44"}]
["01105","01","AL","105","Perry","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",76.65489845160002,"A","CEC Survey",2017,15,"I",42.84033120833613,"TON",8,{"v":0.558872714904,"d":"0.56"},{"$f":"VLOOKUP(A790,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.442321104,"d":"0.44"}]
["01105","01","AL","105","Perry","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,470.887452162,"A","CEC Survey",2017,15,"I",88.14537109563273,"TON",8,{"v":0.1871898915355,"d":"0.19"},{"$f":"VLOOKUP(A791,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.148151873,"d":"0.15"}]
["01105","01","AL","105","Perry","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",122.30226663299999,"A","CEC Survey",2017,15,"I",29.93864592847159,"TON",8,{"v":0.244792241,"d":"0.24"},{"$f":"VLOOKUP(A792,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.19374138583300354,"d":"0.19"}]
["01105","01","AL","105","Perry","","2104009000","Wax Log; Total: All Combustor Types",null,43.649072444850134,"A","CEC Survey",2017,15,"I",10.219657724379385,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A793,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.1853045508508112,"d":"0.19"}]
["01105","01","AL","105","Perry","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",123.22540874151001,"A","CEC Survey",2017,15,"I",120.44916311666331,"TON",8,{"v":0.9774701853034999,"d":"0.98"},{"$f":"VLOOKUP(A794,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.773621041,"d":"0.77"}]
["01105","01","AL","105","Perry","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",162.97554059361,"A","CEC Survey",2017,15,"I",159.30373186397406,"TON",8,{"v":0.9774701853035002,"d":"0.98"},{"$f":"VLOOKUP(A795,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.7736210410000001,"d":"0.77"}]
["01105","01","AL","105","Perry","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",111.30036918588002,"A","CEC Survey",2017,15,"I",108.7927924924701,"TON",8,{"v":0.9774701853034999,"d":"0.98"},{"$f":"VLOOKUP(A796,cordwood_density!A:D,4,FALSE)","v":1.2635},{"v":0.773621041,"d":"0.77"}]
["01107","01","AL","107","Pickens","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",56.57092948113031,"A","CEC Survey",2017,15,"I",86.94528233505518,"TON",8,{"v":1.5369251156471893,"d":"1.54"},{"$f":"VLOOKUP(A797,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":1.2069460622327541,"d":"1.21"}]
["01107","01","AL","107","Pickens","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.586832120091646,"A","CEC Survey",2017,15,"I",7.049617486626095,"TON",8,{"v":1.5369251156471893,"d":"1.54"},{"$f":"VLOOKUP(A798,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":1.2069460622327541,"d":"1.21"}]
["01107","01","AL","107","Pickens","","2104008610","Hydronic heater: outdoor","Hydronic heater",55.041985441099754,"A","CEC Survey",2017,15,"I",84.59540983951315,"TON",8,{"v":1.5369251156471893,"d":"1.54"},{"$f":"VLOOKUP(A799,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":1.2069460622327541,"d":"1.21"}]
["01107","01","AL","107","Pickens","","2104008620","Hydronic heater: indoor","Hydronic heater",35.165712920702624,"A","CEC Survey",2017,15,"I",54.04706739746674,"TON",8,{"v":1.5369251156471893,"d":"1.54"},{"$f":"VLOOKUP(A800,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":1.2069460622327541,"d":"1.21"}]
["01107","01","AL","107","Pickens","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.528944040030549,"A","CEC Survey",2017,15,"I",2.3498724955420323,"TON",8,{"v":1.5369251156471893,"d":"1.54"},{"$f":"VLOOKUP(A801,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":1.2069460622327541,"d":"1.21"}]
["01107","01","AL","107","Pickens","","2104008100","Fireplace: general","Fireplace: general",859.56246426,"A","CEC Survey",2017,15,"I",236.8223700604741,"TON",8,{"v":0.275515020615,"d":"0.28"},{"$f":"VLOOKUP(A802,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.21636172499999998,"d":"0.22"}]
["01107","01","AL","107","Pickens","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",225.77154058199997,"A","CEC Survey",2017,15,"I",137.07024962016908,"TON",8,{"v":0.6071192554510001,"d":"0.61"},{"$f":"VLOOKUP(A803,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.476770265,"d":"0.48"}]
["01107","01","AL","107","Pickens","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",298.601069802,"A","CEC Survey",2017,15,"I",181.2864591750623,"TON",8,{"v":0.607119255451,"d":"0.61"},{"$f":"VLOOKUP(A804,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.47677026499999997,"d":"0.48"}]
["01107","01","AL","107","Pickens","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",203.922681816,"A","CEC Survey",2017,15,"I",123.80538675370111,"TON",8,{"v":0.6071192554510001,"d":"0.61"},{"$f":"VLOOKUP(A805,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.476770265,"d":"0.48"}]
["01107","01","AL","107","Pickens","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1206.5255397,"A","CEC Survey",2017,15,"I",223.04789077165015,"TON",8,{"v":0.18486793974299998,"d":"0.18"},{"$f":"VLOOKUP(A806,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.14517664499999997,"d":"0.15"}]
["01107","01","AL","107","Pickens","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",306.53129448000004,"A","CEC Survey",2017,15,"I",95.83853114704911,"TON",8,{"v":0.312654965,"d":"0.31"},{"$f":"VLOOKUP(A807,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.24552769357625254,"d":"0.25"}]
["01107","01","AL","107","Pickens","","2104009000","Wax Log; Total: All Combustor Types",null,109.44584798610003,"A","CEC Survey",2017,15,"I",25.624808114435968,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A808,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.18386390764881416,"d":"0.18"}]
["01107","01","AL","107","Pickens","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",342.3840640494,"A","CEC Survey",2017,15,"I",352.2716249525639,"TON",8,{"v":1.0288785663276,"d":"1.03"},{"$f":"VLOOKUP(A809,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.8079775140000001,"d":"0.81"}]
["01107","01","AL","107","Pickens","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",452.8305363234,"A","CEC Survey",2017,15,"I",465.90763300177804,"TON",8,{"v":1.0288785663276,"d":"1.03"},{"$f":"VLOOKUP(A810,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.8079775140000001,"d":"0.81"}]
["01107","01","AL","107","Pickens","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",309.25012236720005,"A","CEC Survey",2017,15,"I",318.18082253779966,"TON",8,{"v":1.0288785663276,"d":"1.03"},{"$f":"VLOOKUP(A811,cordwood_density!A:D,4,FALSE)","v":1.2734},{"v":0.8079775140000001,"d":"0.81"}]
["01109","01","AL","109","Pike","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",41.30742716413126,"A","CEC Survey",2017,15,"I",64.30719158442365,"TON",8,{"v":1.5567948913619079,"d":"1.56"},{"$f":"VLOOKUP(A812,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":1.1743191456301636,"d":"1.17"}]
["01109","01","AL","109","Pike","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.349250851145778,"A","CEC Survey",2017,15,"I",5.214096614953269,"TON",8,{"v":1.556794891361908,"d":"1.56"},{"$f":"VLOOKUP(A813,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":1.1743191456301636,"d":"1.17"}]
["01109","01","AL","109","Pike","","2104008610","Hydronic heater: outdoor","Hydronic heater",40.19101021374933,"A","CEC Survey",2017,15,"I",62.56915937943923,"TON",8,{"v":1.556794891361908,"d":"1.56"},{"$f":"VLOOKUP(A814,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":1.1743191456301636,"d":"1.17"}]
["01109","01","AL","109","Pike","","2104008620","Hydronic heater: indoor","Hydronic heater",25.677589858784298,"A","CEC Survey",2017,15,"I",39.97474071464173,"TON",8,{"v":1.556794891361908,"d":"1.56"},{"$f":"VLOOKUP(A815,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":1.1743191456301636,"d":"1.17"}]
["01109","01","AL","109","Pike","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.116416950381926,"A","CEC Survey",2017,15,"I",1.738032204984423,"TON",8,{"v":1.556794891361908,"d":"1.56"},{"$f":"VLOOKUP(A816,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":1.1743191456301636,"d":"1.17"}]
["01109","01","AL","109","Pike","","2104008100","Fireplace: general","Fireplace: general",1098.856449224,"A","CEC Survey",2017,15,"I",284.91475782572695,"TON",8,{"v":0.259282964601,"d":"0.26"},{"$f":"VLOOKUP(A817,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.19558192999999996,"d":"0.20"}]
["01109","01","AL","109","Pike","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",319.80189529231995,"A","CEC Survey",2017,15,"I",181.23767511931428,"TON",8,{"v":0.5667185773044,"d":"0.57"},{"$f":"VLOOKUP(A818,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.427486292,"d":"0.43"}]
["01109","01","AL","109","Pike","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",422.96379699951996,"A","CEC Survey",2017,15,"I",239.701441286835,"TON",8,{"v":0.5667185773044,"d":"0.57"},{"$f":"VLOOKUP(A819,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.427486292,"d":"0.43"}]
["01109","01","AL","109","Pike","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",288.85332478016,"A","CEC Survey",2017,15,"I",163.6985452690581,"TON",8,{"v":0.5667185773044001,"d":"0.57"},{"$f":"VLOOKUP(A820,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.42748629200000005,"d":"0.43"}]
["01109","01","AL","109","Pike","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1551.7328023559999,"A","CEC Survey",2017,15,"I",300.20856948303594,"TON",8,{"v":0.19346666451030003,"d":"0.19"},{"$f":"VLOOKUP(A821,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.145935479,"d":"0.15"}]
["01109","01","AL","109","Pike","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",339.964109956,"A","CEC Survey",2017,15,"I",71.12143316341567,"TON",8,{"v":0.209202769,"d":"0.21"},{"$f":"VLOOKUP(A822,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.15780551331372106,"d":"0.16"}]
["01109","01","AL","109","Pike","","2104009000","Wax Log; Total: All Combustor Types",null,176.43475021801217,"A","CEC Survey",2017,15,"I",41.30907386846869,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A823,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.17661031907671418,"d":"0.18"}]
["01109","01","AL","109","Pike","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",367.42567384084003,"A","CEC Survey",2017,15,"I",340.20387889438047,"TON",8,{"v":0.9259121044485003,"d":"0.93"},{"$f":"VLOOKUP(A824,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.6984326050000002,"d":"0.70"}]
["01109","01","AL","109","Pike","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",485.95008475724,"A","CEC Survey",2017,15,"I",449.94706563450313,"TON",8,{"v":0.9259121044485003,"d":"0.93"},{"$f":"VLOOKUP(A825,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.6984326050000002,"d":"0.70"}]
["01109","01","AL","109","Pike","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",331.86835056592,"A","CEC Survey",2017,15,"I",307.28092287234364,"TON",8,{"v":0.9259121044485003,"d":"0.93"},{"$f":"VLOOKUP(A826,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.6984326050000002,"d":"0.70"}]
["01111","01","AL","111","Randolph","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",55.48713071778734,"A","CEC Survey",2017,15,"I",88.40542670521579,"TON",8,{"v":1.5932600147384435,"d":"1.59"},{"$f":"VLOOKUP(A827,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":1.2503021382236863,"d":"1.25"}]
["01111","01","AL","111","Randolph","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.49895654468546,"A","CEC Survey",2017,15,"I",7.168007570693172,"TON",8,{"v":1.5932600147384433,"d":"1.59"},{"$f":"VLOOKUP(A828,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":1.250302138223686,"d":"1.25"}]
["01111","01","AL","111","Randolph","","2104008610","Hydronic heater: outdoor","Hydronic heater",53.98747853622552,"A","CEC Survey",2017,15,"I",86.01609084831806,"TON",8,{"v":1.5932600147384433,"d":"1.59"},{"$f":"VLOOKUP(A829,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":1.250302138223686,"d":"1.25"}]
["01111","01","AL","111","Randolph","","2104008620","Hydronic heater: indoor","Hydronic heater",34.49200017592186,"A","CEC Survey",2017,15,"I",54.95472470864765,"TON",8,{"v":1.5932600147384435,"d":"1.59"},{"$f":"VLOOKUP(A830,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":1.2503021382236863,"d":"1.25"}]
["01111","01","AL","111","Randolph","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.49965218156182,"A","CEC Survey",2017,15,"I",2.389335856897724,"TON",8,{"v":1.5932600147384433,"d":"1.59"},{"$f":"VLOOKUP(A831,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":1.250302138223686,"d":"1.25"}]
["01111","01","AL","111","Randolph","","2104008100","Fireplace: general","Fireplace: general",865.1834529734265,"A","CEC Survey",2017,15,"I",231.2825646465413,"TON",8,{"v":0.2673219926383,"d":"0.27"},{"$f":"VLOOKUP(A832,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.209779481,"d":"0.21"}]
["01111","01","AL","111","Randolph","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",282.29419022675347,"A","CEC Survey",2017,15,"I",156.2358577682937,"TON",8,{"v":0.5534504895152,"d":"0.55"},{"$f":"VLOOKUP(A833,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.43431726400000004,"d":"0.43"}]
["01111","01","AL","111","Randolph","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",373.3568322353836,"A","CEC Survey",2017,15,"I",206.63452156451746,"TON",8,{"v":0.5534504895152,"d":"0.55"},{"$f":"VLOOKUP(A834,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.43431726400000004,"d":"0.43"}]
["01111","01","AL","111","Randolph","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",254.97539762416446,"A","CEC Survey",2017,15,"I",141.11625862942657,"TON",8,{"$f":"P835/J835","v":{"v":0.5534504895151999,"d":"0.55"}},{"$f":"VLOOKUP(A835,cordwood_density!A:D,4,FALSE)","v":1.2743},{"$f":"S835/T835","v":{"v":0.4343172639999999,"d":"0.43"}}]
["01111","01","AL","111","Randolph","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1396.1846700815413,"A","CEC Survey",2017,15,"I",262.51297551078125,"TON",8,{"v":0.1880216715855,"d":"0.19"},{"$f":"VLOOKUP(A836,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.14754898500000002,"d":"0.15"}]
["01111","01","AL","111","Randolph","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",344.57270173513984,"A","CEC Survey",2017,15,"I",98.14950076574165,"TON",8,{"v":0.284844099,"d":"0.28"},{"$f":"VLOOKUP(A837,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.2235298587459782,"d":"0.22"}]
["01111","01","AL","111","Randolph","","2104009000","Wax Log; Total: All Combustor Types",null,127.35647427602403,"A","CEC Survey",2017,15,"I",43.73787476502209,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A838,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.2695038452483717,"d":"0.27"}]
["01111","01","AL","111","Randolph","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",397.22194066349226,"A","CEC Survey",2017,15,"I",383.4004298804411,"TON",8,{"v":0.9652045635747999,"d":"0.97"},{"$f":"VLOOKUP(A839,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.757439036,"d":"0.76"}]
["01111","01","AL","111","Randolph","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",525.3580505549413,"A","CEC Survey",2017,15,"I",507.0779879063898,"TON",8,{"v":0.9652045635747999,"d":"0.97"},{"$f":"VLOOKUP(A840,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.757439036,"d":"0.76"}]
["01111","01","AL","111","Randolph","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",358.7811076960575,"A","CEC Survey",2017,15,"I",346.2971624726565,"TON",8,{"v":0.9652045635748,"d":"0.97"},{"$f":"VLOOKUP(A841,cordwood_density!A:D,4,FALSE)","v":1.2743},{"v":0.757439036,"d":"0.76"}]
["01113","01","AL","113","Russell","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",68.58718287878374,"A","CEC Survey",2017,15,"I",97.35544232840385,"TON",8,{"v":1.4194407503288649,"d":"1.42"},{"$f":"VLOOKUP(A842,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":1.1562730126497758,"d":"1.16"}]
["01113","01","AL","113","Russell","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.5611229361176,"A","CEC Survey",2017,15,"I",7.893684513113826,"TON",8,{"v":1.4194407503288649,"d":"1.42"},{"$f":"VLOOKUP(A843,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":1.1562730126497758,"d":"1.16"}]
["01113","01","AL","113","Russell","","2104008610","Hydronic heater: outdoor","Hydronic heater",66.7334752334112,"A","CEC Survey",2017,15,"I",94.7242141573659,"TON",8,{"v":1.4194407503288649,"d":"1.42"},{"$f":"VLOOKUP(A844,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":1.1562730126497758,"d":"1.16"}]
["01113","01","AL","113","Russell","","2104008620","Hydronic heater: indoor","Hydronic heater",42.635275843568266,"A","CEC Survey",2017,15,"I",60.51824793387267,"TON",8,{"v":1.419440750328865,"d":"1.42"},{"$f":"VLOOKUP(A845,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":1.156273012649776,"d":"1.16"}]
["01113","01","AL","113","Russell","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.8537076453725334,"A","CEC Survey",2017,15,"I",2.631228171037942,"TON",8,{"v":1.4194407503288649,"d":"1.42"},{"$f":"VLOOKUP(A846,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":1.1562730126497758,"d":"1.16"}]
["01113","01","AL","113","Russell","","2104008100","Fireplace: general","Fireplace: general",2436.27980138,"A","CEC Survey",2017,15,"I",554.742125126199,"TON",8,{"v":0.22770049844520002,"d":"0.23"},{"$f":"VLOOKUP(A847,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.185484277,"d":"0.19"}]
["01113","01","AL","113","Russell","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",603.2120285726,"A","CEC Survey",2017,15,"I",330.4420439034568,"TON",8,{"v":0.5478041356128001,"d":"0.55"},{"$f":"VLOOKUP(A848,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.44623992800000006,"d":"0.45"}]
["01113","01","AL","113","Russell","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",797.7965539186,"A","CEC Survey",2017,15,"I",437.0362516142493,"TON",8,{"v":0.5478041356128001,"d":"0.55"},{"$f":"VLOOKUP(A849,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.44623992800000006,"d":"0.45"}]
["01113","01","AL","113","Russell","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",544.8366709688,"A","CEC Survey",2017,15,"I",298.46378159021907,"TON",8,{"v":0.5478041356128001,"d":"0.55"},{"$f":"VLOOKUP(A850,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.44623992800000006,"d":"0.45"}]
["01113","01","AL","113","Russell","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3085.02204819,"A","CEC Survey",2017,15,"I",555.6335020308596,"TON",8,{"v":0.18010681718040003,"d":"0.18"},{"$f":"VLOOKUP(A851,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.146714579,"d":"0.15"}]
["01113","01","AL","113","Russell","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",636.8897395800001,"A","CEC Survey",2017,15,"I",120.77707489657332,"TON",8,{"v":0.189635768,"d":"0.19"},{"$f":"VLOOKUP(A852,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.1544768393613555,"d":"0.15"}]
["01113","01","AL","113","Russell","","2104009000","Wax Log; Total: All Combustor Types",null,325.895838688269,"A","CEC Survey",2017,15,"I",76.3027422725134,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A853,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.19072360703812316,"d":"0.19"}]
["01113","01","AL","113","Russell","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",635.4621435471,"A","CEC Survey",2017,15,"I",503.08958759753625,"TON",8,{"v":0.7916908862412,"d":"0.79"},{"$f":"VLOOKUP(A854,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.644909487,"d":"0.64"}]
["01113","01","AL","113","Russell","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",840.4499317880999,"A","CEC Survey",2017,15,"I",665.3765513386769,"TON",8,{"v":0.7916908862412,"d":"0.79"},{"$f":"VLOOKUP(A855,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.644909487,"d":"0.64"}]
["01113","01","AL","113","Russell","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",573.9658070748001,"A","CEC Survey",2017,15,"I",454.40349847519406,"TON",8,{"v":0.7916908862412,"d":"0.79"},{"$f":"VLOOKUP(A856,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.644909487,"d":"0.64"}]
["01115","01","AL","115","St Clair","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",178.43452496414758,"A","CEC Survey",2017,15,"I",300.1539836947639,"TON",8,{"v":1.6821519476405875,"d":"1.68"},{"$f":"VLOOKUP(A857,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":1.2317141009303563,"d":"1.23"}]
["01115","01","AL","115","St Clair","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.467664186282237,"A","CEC Survey",2017,15,"I",24.336809488764636,"TON",8,{"v":1.6821519476405873,"d":"1.68"},{"$f":"VLOOKUP(A858,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":1.231714100930356,"d":"1.23"}]
["01115","01","AL","115","St Clair","","2104008610","Hydronic heater: outdoor","Hydronic heater",173.61197023538685,"A","CEC Survey",2017,15,"I",292.04171386517567,"TON",8,{"v":1.6821519476405873,"d":"1.68"},{"$f":"VLOOKUP(A859,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":1.231714100930356,"d":"1.23"}]
["01115","01","AL","115","St Clair","","2104008620","Hydronic heater: indoor","Hydronic heater",110.91875876149716,"A","CEC Survey",2017,15,"I",186.5822060805289,"TON",8,{"v":1.6821519476405873,"d":"1.68"},{"$f":"VLOOKUP(A860,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":1.231714100930356,"d":"1.23"}]
["01115","01","AL","115","St Clair","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.822554728760746,"A","CEC Survey",2017,15,"I",8.112269829588213,"TON",8,{"v":1.682151947640587,"d":"1.68"},{"$f":"VLOOKUP(A861,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":1.231714100930356,"d":"1.23"}]
["01115","01","AL","115","St Clair","","2104008100","Fireplace: general","Fireplace: general",3639.198767058,"A","CEC Survey",2017,15,"I",987.9260237617243,"TON",8,{"v":0.27146800353539996,"d":"0.27"},{"$f":"VLOOKUP(A862,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.198775722,"d":"0.20"}]
["01115","01","AL","115","St Clair","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",888.45694884856,"A","CEC Survey",2017,15,"I",509.4555063338616,"TON",8,{"v":0.5734160861638999,"d":"0.57"},{"$f":"VLOOKUP(A863,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.41986972699999997,"d":"0.42"}]
["01115","01","AL","115","St Clair","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1175.05596460616,"A","CEC Survey",2017,15,"I",673.7959922480104,"TON",8,{"v":0.5734160861638999,"d":"0.57"},{"$f":"VLOOKUP(A864,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.41986972699999997,"d":"0.42"}]
["01115","01","AL","115","St Clair","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",802.47724412128,"A","CEC Survey",2017,15,"I",460.15336055961694,"TON",8,{"v":0.5734160861639,"d":"0.57"},{"$f":"VLOOKUP(A865,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.4198697270000001,"d":"0.42"}]
["01115","01","AL","115","St Clair","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4885.580455296001,"A","CEC Survey",2017,15,"I",988.3688825548069,"TON",8,{"v":0.20230326602919999,"d":"0.20"},{"$f":"VLOOKUP(A866,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.148131556,"d":"0.15"}]
["01115","01","AL","115","St Clair","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1158.977455518,"A","CEC Survey",2017,15,"I",311.8047545227812,"TON",8,{"v":0.269034357,"d":"0.27"},{"$f":"VLOOKUP(A867,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.19699374459983893,"d":"0.20"}]
["01115","01","AL","115","St Clair","","2104009000","Wax Log; Total: All Combustor Types",null,272.24145122,"A","CEC Survey",2017,15,"I",93.49554129067057,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A868,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.25146719630958486,"d":"0.25"}]
["01115","01","AL","115","St Clair","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1228.12130731314,"A","CEC Survey",2017,15,"I",1228.1783798075542,"TON",8,{"v":1.0000464713819996,"d":"1.00"},{"$f":"VLOOKUP(A869,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.7322592599999997,"d":"0.73"}]
["01115","01","AL","115","St Clair","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1624.28947096254,"A","CEC Survey",2017,15,"I",1624.3649539390233,"TON",8,{"v":1.0000464713819996,"d":"1.00"},{"$f":"VLOOKUP(A870,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.7322592599999997,"d":"0.73"}]
["01115","01","AL","115","St Clair","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1109.2708582183202,"A","CEC Survey",2017,15,"I",1109.3224075681137,"TON",8,{"v":1.0000464713819999,"d":"1.00"},{"$f":"VLOOKUP(A871,cordwood_density!A:D,4,FALSE)","v":1.3657},{"v":0.73225926,"d":"0.73"}]
["01117","01","AL","117","Shelby","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",256.5077231787147,"A","CEC Survey",2017,15,"I",393.1818198845155,"TON",8,{"v":1.5328264389551223,"d":"1.53"},{"$f":"VLOOKUP(A872,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":1.1728720169524236,"d":"1.17"}]
["01117","01","AL","117","Shelby","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",20.797923500976868,"A","CEC Survey",2017,15,"I",31.879607017663417,"TON",8,{"v":1.532826438955122,"d":"1.53"},{"$f":"VLOOKUP(A873,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":1.1728720169524234,"d":"1.17"}]
["01117","01","AL","117","Shelby","","2104008610","Hydronic heater: outdoor","Hydronic heater",249.5750820117224,"A","CEC Survey",2017,15,"I",382.555284211961,"TON",8,{"v":1.532826438955122,"d":"1.53"},{"$f":"VLOOKUP(A874,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":1.1728720169524234,"d":"1.17"}]
["01117","01","AL","117","Shelby","","2104008620","Hydronic heater: indoor","Hydronic heater",159.45074684082266,"A","CEC Survey",2017,15,"I",244.4103204687529,"TON",8,{"v":1.5328264389551223,"d":"1.53"},{"$f":"VLOOKUP(A875,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":1.1728720169524236,"d":"1.17"}]
["01117","01","AL","117","Shelby","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",6.93264116699229,"A","CEC Survey",2017,15,"I",10.626535672554473,"TON",8,{"v":1.532826438955122,"d":"1.53"},{"$f":"VLOOKUP(A876,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":1.1728720169524234,"d":"1.17"}]
["01117","01","AL","117","Shelby","","2104008100","Fireplace: general","Fireplace: general",12141.240412356,"A","CEC Survey",2017,15,"I",2713.959967340784,"TON",8,{"v":0.22353234720390003,"d":"0.22"},{"$f":"VLOOKUP(A877,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.17104013100000004,"d":"0.17"}]
["01117","01","AL","117","Shelby","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1705.19604943864,"A","CEC Survey",2017,15,"I",1002.5841266342125,"TON",8,{"v":0.5879582743369999,"d":"0.59"},{"$f":"VLOOKUP(A878,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.44988772999999993,"d":"0.45"}]
["01117","01","AL","117","Shelby","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2255.25929119304,"A","CEC Survey",2017,15,"I",1325.9983610323454,"TON",8,{"v":0.5879582743369999,"d":"0.59"},{"$f":"VLOOKUP(A879,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.44988772999999993,"d":"0.45"}]
["01117","01","AL","117","Shelby","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1540.1770769123202,"A","CEC Survey",2017,15,"I",905.5598563147727,"TON",8,{"v":0.587958274337,"d":"0.59"},{"$f":"VLOOKUP(A880,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.44988773,"d":"0.45"}]
["01117","01","AL","117","Shelby","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,11200.301222924,"A","CEC Survey",2017,15,"I",2171.9799119153968,"TON",8,{"v":0.19392156234779998,"d":"0.19"},{"$f":"VLOOKUP(A881,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.14838286199999998,"d":"0.15"}]
["01117","01","AL","117","Shelby","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2217.459776576,"A","CEC Survey",2017,15,"I",450.2837241664836,"TON",8,{"v":0.20306286,"d":"0.20"},{"$f":"VLOOKUP(A882,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.15537750401713982,"d":"0.16"}]
["01117","01","AL","117","Shelby","","2104009000","Wax Log; Total: All Combustor Types",null,644.17459436,"A","CEC Survey",2017,15,"I",221.22807572281187,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A883,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.26278119978575254,"d":"0.26"}]
["01117","01","AL","117","Shelby","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1933.556485443,"A","CEC Survey",2017,15,"I",1530.5913326300742,"TON",8,{"v":0.7915938035187,"d":"0.79"},{"$f":"VLOOKUP(A884,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.605703423,"d":"0.61"}]
["01117","01","AL","117","Shelby","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2557.2843839729994,"A","CEC Survey",2017,15,"I",2024.3304721881627,"TON",8,{"v":0.7915938035187002,"d":"0.79"},{"$f":"VLOOKUP(A885,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.6057034230000002,"d":"0.61"}]
["01117","01","AL","117","Shelby","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1746.4381158840001,"A","CEC Survey",2017,15,"I",1382.4695907626478,"TON",8,{"v":0.7915938035187,"d":"0.79"},{"$f":"VLOOKUP(A886,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.605703423,"d":"0.61"}]
["01119","01","AL","119","Sumter","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",26.590000506033473,"A","CEC Survey",2017,15,"I",42.63170309761441,"TON",8,{"v":1.6032983184013463,"d":"1.60"},{"$f":"VLOOKUP(A887,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":1.2349212958494542,"d":"1.23"}]
["01119","01","AL","119","Sumter","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.155945986975687,"A","CEC Survey",2017,15,"I",3.4566245754822496,"TON",8,{"v":1.6032983184013463,"d":"1.60"},{"$f":"VLOOKUP(A888,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":1.2349212958494542,"d":"1.23"}]
["01119","01","AL","119","Sumter","","2104008610","Hydronic heater: outdoor","Hydronic heater",25.871351843708243,"A","CEC Survey",2017,15,"I",41.47949490578699,"TON",8,{"v":1.603298318401346,"d":"1.60"},{"$f":"VLOOKUP(A889,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":1.234921295849454,"d":"1.23"}]
["01119","01","AL","119","Sumter","","2104008620","Hydronic heater: indoor","Hydronic heater",16.528919233480266,"A","CEC Survey",2017,15,"I",26.50078841203058,"TON",8,{"v":1.6032983184013463,"d":"1.60"},{"$f":"VLOOKUP(A890,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":1.2349212958494542,"d":"1.23"}]
["01119","01","AL","119","Sumter","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7186486623252291,"A","CEC Survey",2017,15,"I",1.1522081918274165,"TON",8,{"v":1.603298318401346,"d":"1.60"},{"$f":"VLOOKUP(A891,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":1.234921295849454,"d":"1.23"}]
["01119","01","AL","119","Sumter","","2104008100","Fireplace: general","Fireplace: general",399.32140798728494,"A","CEC Survey",2017,15,"I",113.18616926755561,"TON",8,{"v":0.28344628413,"d":"0.28"},{"$f":"VLOOKUP(A892,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.2183211,"d":"0.22"}]
["01119","01","AL","119","Sumter","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",142.94604222629218,"A","CEC Survey",2017,15,"I",78.74322292672488,"TON",8,{"v":0.5508597628892,"d":"0.55"},{"$f":"VLOOKUP(A893,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.424293124,"d":"0.42"}]
["01119","01","AL","119","Sumter","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",189.05766875090254,"A","CEC Survey",2017,15,"I",104.1442625805071,"TON",8,{"v":0.5508597628892001,"d":"0.55"},{"$f":"VLOOKUP(A894,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.4242931240000001,"d":"0.42"}]
["01119","01","AL","119","Sumter","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",129.11255426890907,"A","CEC Survey",2017,15,"I",71.12291103059022,"TON",8,{"v":0.5508597628892,"d":"0.55"},{"$f":"VLOOKUP(A895,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.424293124,"d":"0.42"}]
["01119","01","AL","119","Sumter","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,664.2544904470608,"A","CEC Survey",2017,15,"I",126.23156931798992,"TON",8,{"v":0.19003495066030002,"d":"0.19"},{"$f":"VLOOKUP(A896,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.146372141,"d":"0.15"}]
["01119","01","AL","119","Sumter","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",166.79611561812078,"A","CEC Survey",2017,15,"I",46.220541009036296,"TON",8,{"v":0.277108018,"d":"0.28"},{"$f":"VLOOKUP(A897,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.213439126550104,"d":"0.21"}]
["01119","01","AL","119","Sumter","","2104009000","Wax Log; Total: All Combustor Types",null,72.86335783780046,"A","CEC Survey",2017,15,"I",17.05966555628725,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A898,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.18033759531695295,"d":"0.18"}]
["01119","01","AL","119","Sumter","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",203.4144756188225,"A","CEC Survey",2017,15,"I",209.7279282207149,"TON",8,{"$f":"P899/J899","v":{"v":1.0310373811042,"d":"1.03"}},{"$f":"VLOOKUP(A899,cordwood_density!A:D,4,FALSE)","v":1.2983},{"$f":"S899/T899","v":{"v":0.7941441739999999,"d":"0.79"}}]
["01119","01","AL","119","Sumter","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",269.0320483990878,"A","CEC Survey",2017,15,"I",277.3820986144939,"TON",8,{"v":1.0310373811042002,"d":"1.03"},{"$f":"VLOOKUP(A900,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.7941441740000001,"d":"0.79"}]
["01119","01","AL","119","Sumter","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",183.7292037847429,"A","CEC Survey",2017,15,"I",189.4316771025812,"TON",8,{"v":1.0310373811042,"d":"1.03"},{"$f":"VLOOKUP(A901,cordwood_density!A:D,4,FALSE)","v":1.2983},{"v":0.7941441739999999,"d":"0.79"}]
["01121","01","AL","121","Talladega","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",146.22674595545098,"A","CEC Survey",2017,15,"I",232.6813815869297,"TON",8,{"v":1.591236815581041,"d":"1.59"},{"$f":"VLOOKUP(A902,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":1.2209290382728775,"d":"1.22"}]
["01121","01","AL","121","Talladega","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.856222645036565,"A","CEC Survey",2017,15,"I",18.866057966507814,"TON",8,{"v":1.5912368155810412,"d":"1.59"},{"$f":"VLOOKUP(A903,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":1.2209290382728777,"d":"1.22"}]
["01121","01","AL","121","Talladega","","2104008610","Hydronic heater: outdoor","Hydronic heater",142.27467174043878,"A","CEC Survey",2017,15,"I",226.39269559809375,"TON",8,{"v":1.5912368155810412,"d":"1.59"},{"$f":"VLOOKUP(A904,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":1.2209290382728777,"d":"1.22"}]
["01121","01","AL","121","Talladega","","2104008620","Hydronic heater: indoor","Hydronic heater",90.89770694528033,"A","CEC Survey",2017,15,"I",144.63977774322657,"TON",8,{"v":1.5912368155810412,"d":"1.59"},{"$f":"VLOOKUP(A905,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":1.2209290382728777,"d":"1.22"}]
["01121","01","AL","121","Talladega","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.9520742150121886,"A","CEC Survey",2017,15,"I",6.288685988835938,"TON",8,{"v":1.591236815581041,"d":"1.59"},{"$f":"VLOOKUP(A906,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":1.2209290382728775,"d":"1.22"}]
["01121","01","AL","121","Talladega","","2104008100","Fireplace: general","Fireplace: general",3299.9688673749997,"A","CEC Survey",2017,15,"I",834.5675949754972,"TON",8,{"v":0.2529016571115,"d":"0.25"},{"$f":"VLOOKUP(A907,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.194047155,"d":"0.19"}]
["01121","01","AL","121","Talladega","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",824.4504536399701,"A","CEC Survey",2017,15,"I",440.427822752912,"TON",8,{"v":0.5342077511248999,"d":"0.53"},{"$f":"VLOOKUP(A908,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.409888553,"d":"0.41"}]
["01121","01","AL","121","Talladega","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1090.40221287867,"A","CEC Survey",2017,15,"I",582.5013139635287,"TON",8,{"v":0.5342077511248998,"d":"0.53"},{"$f":"VLOOKUP(A909,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.4098885529999999,"d":"0.41"}]
["01121","01","AL","121","Talladega","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",744.6649258683601,"A","CEC Survey",2017,15,"I",397.805775389727,"TON",8,{"v":0.5342077511248999,"d":"0.53"},{"$f":"VLOOKUP(A910,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.409888553,"d":"0.41"}]
["01121","01","AL","121","Talladega","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4448.604008968,"A","CEC Survey",2017,15,"I",851.6206837342875,"TON",8,{"v":0.19143548897979995,"d":"0.19"},{"$f":"VLOOKUP(A911,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.14688520599999996,"d":"0.15"}]
["01121","01","AL","121","Talladega","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",999.414444778,"A","CEC Survey",2017,15,"I",249.56451257688795,"TON",8,{"v":0.249710732,"d":"0.25"},{"$f":"VLOOKUP(A912,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.1915988122458375,"d":"0.19"}]
["01121","01","AL","121","Talladega","","2104009000","Wax Log; Total: All Combustor Types",null,454.6024323632614,"A","CEC Survey",2017,15,"I",156.1235450934744,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A913,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.2635070590040666,"d":"0.26"}]
["01121","01","AL","121","Talladega","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1075.59894870728,"A","CEC Survey",2017,15,"I",998.7813536546668,"TON",8,{"v":0.9285815636535,"d":"0.93"},{"$f":"VLOOKUP(A914,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.712484895,"d":"0.71"}]
["01121","01","AL","121","Talladega","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1422.56635151608,"A","CEC Survey",2017,15,"I",1320.968887091656,"TON",8,{"v":0.9285815636534999,"d":"0.93"},{"$f":"VLOOKUP(A915,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.7124848949999999,"d":"0.71"}]
["01121","01","AL","121","Talladega","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",971.50872786464,"A","CEC Survey",2017,15,"I",902.12509362357,"TON",8,{"v":0.9285815636535,"d":"0.93"},{"$f":"VLOOKUP(A916,cordwood_density!A:D,4,FALSE)","v":1.3033},{"v":0.712484895,"d":"0.71"}]
["01123","01","AL","123","Tallapoosa","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",96.94379520667465,"A","CEC Survey",2017,15,"I",152.2205496378749,"TON",8,{"v":1.5701938356483327,"d":"1.57"},{"$f":"VLOOKUP(A917,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":1.2226067395844684,"d":"1.22"}]
["01123","01","AL","123","Tallapoosa","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.860307719460106,"A","CEC Survey",2017,15,"I",12.342206727395261,"TON",8,{"v":1.5701938356483325,"d":"1.57"},{"$f":"VLOOKUP(A918,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":1.2226067395844682,"d":"1.22"}]
["01123","01","AL","123","Tallapoosa","","2104008610","Hydronic heater: outdoor","Hydronic heater",94.32369263352128,"A","CEC Survey",2017,15,"I",148.10648072874315,"TON",8,{"v":1.5701938356483327,"d":"1.57"},{"$f":"VLOOKUP(A919,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":1.2226067395844684,"d":"1.22"}]
["01123","01","AL","123","Tallapoosa","","2104008620","Hydronic heater: indoor","Hydronic heater",60.26235918252749,"A","CEC Survey",2017,15,"I",94.62358491003035,"TON",8,{"v":1.5701938356483325,"d":"1.57"},{"$f":"VLOOKUP(A920,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":1.2226067395844682,"d":"1.22"}]
["01123","01","AL","123","Tallapoosa","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.620102573153369,"A","CEC Survey",2017,15,"I",4.114068909131754,"TON",8,{"v":1.5701938356483327,"d":"1.57"},{"$f":"VLOOKUP(A921,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":1.2226067395844684,"d":"1.22"}]
["01123","01","AL","123","Tallapoosa","","2104008100","Fireplace: general","Fireplace: general",1822.386403854,"A","CEC Survey",2017,15,"I",477.19609967309157,"TON",8,{"v":0.2618523155484,"d":"0.26"},{"$f":"VLOOKUP(A922,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.203887188,"d":"0.20"}]
["01123","01","AL","123","Tallapoosa","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",483.56730355227995,"A","CEC Survey",2017,15,"I",284.1220897254755,"TON",8,{"v":0.5875543851669,"d":"0.59"},{"$f":"VLOOKUP(A923,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.457489983,"d":"0.46"}]
["01123","01","AL","123","Tallapoosa","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",639.5567563110799,"A","CEC Survey",2017,15,"I",375.77437673369343,"TON",8,{"v":0.5875543851669,"d":"0.59"},{"$f":"VLOOKUP(A924,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.457489983,"d":"0.46"}]
["01123","01","AL","123","Tallapoosa","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",436.77046772464,"A","CEC Survey",2017,15,"I",256.62640362301016,"TON",8,{"v":0.5875543851669,"d":"0.59"},{"$f":"VLOOKUP(A925,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.457489983,"d":"0.46"}]
["01123","01","AL","123","Tallapoosa","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2542.1472445219997,"A","CEC Survey",2017,15,"I",480.0442056992211,"TON",8,{"v":0.1888341466977,"d":"0.19"},{"$f":"VLOOKUP(A926,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.147032739,"d":"0.15"}]
["01123","01","AL","123","Tallapoosa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",611.149170023,"A","CEC Survey",2017,15,"I",169.70212981054274,"TON",8,{"v":0.277677101,"d":"0.28"},{"$f":"VLOOKUP(A927,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.21620890835474577,"d":"0.22"}]
["01123","01","AL","123","Tallapoosa","","2104009000","Wax Log; Total: All Combustor Types",null,235.10749155964191,"A","CEC Survey",2017,15,"I",80.74267194196338,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A928,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.2674053959355291,"d":"0.27"}]
["01123","01","AL","123","Tallapoosa","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",663.66318945688,"A","CEC Survey",2017,15,"I",634.9119084979351,"TON",8,{"v":0.9566779031658001,"d":"0.96"},{"$f":"VLOOKUP(A929,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.7449022060000001,"d":"0.74"}]
["01123","01","AL","123","Tallapoosa","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",877.74808928168,"A","CEC Survey",2017,15,"I",839.722201561785,"TON",8,{"v":0.9566779031658,"d":"0.96"},{"$f":"VLOOKUP(A930,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.744902206,"d":"0.74"}]
["01123","01","AL","123","Tallapoosa","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",599.4377195094401,"A","CEC Survey",2017,15,"I",573.4688205787802,"TON",8,{"v":0.9566779031658001,"d":"0.96"},{"$f":"VLOOKUP(A931,cordwood_density!A:D,4,FALSE)","v":1.2843},{"v":0.7449022060000001,"d":"0.74"}]
["01125","01","AL","125","Tuscaloosa","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",216.75622630650327,"A","CEC Survey",2017,15,"I",331.3035641587469,"TON",8,{"v":1.5284615801082846,"d":"1.53"},{"$f":"VLOOKUP(A932,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":1.1798236820596562,"d":"1.18"}]
["01125","01","AL","125","Tuscaloosa","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",17.574829159986752,"A","CEC Survey",2017,15,"I",26.862451148006503,"TON",8,{"v":1.5284615801082844,"d":"1.53"},{"$f":"VLOOKUP(A933,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":1.179823682059656,"d":"1.18"}]
["01125","01","AL","125","Tuscaloosa","","2104008610","Hydronic heater: outdoor","Hydronic heater",210.897949919841,"A","CEC Survey",2017,15,"I",322.34941377607805,"TON",8,{"v":1.5284615801082846,"d":"1.53"},{"$f":"VLOOKUP(A934,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":1.1798236820596562,"d":"1.18"}]
["01125","01","AL","125","Tuscaloosa","","2104008620","Hydronic heater: indoor","Hydronic heater",134.74035689323176,"A","CEC Survey",2017,15,"I",205.9454588013832,"TON",8,{"v":1.5284615801082846,"d":"1.53"},{"$f":"VLOOKUP(A935,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":1.1798236820596562,"d":"1.18"}]
["01125","01","AL","125","Tuscaloosa","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.858276386662251,"A","CEC Survey",2017,15,"I",8.954150382668836,"TON",8,{"v":1.5284615801082846,"d":"1.53"},{"$f":"VLOOKUP(A936,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":1.1798236820596562,"d":"1.18"}]
["01125","01","AL","125","Tuscaloosa","","2104008100","Fireplace: general","Fireplace: general",9304.819198842755,"A","CEC Survey",2017,15,"I",1991.9351836876062,"TON",8,{"v":0.214075646299,"d":"0.21"},{"$f":"VLOOKUP(A937,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.16524557799999998,"d":"0.17"}]
["01125","01","AL","125","Tuscaloosa","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1546.4052540167706,"A","CEC Survey",2017,15,"I",971.0029171005076,"TON",8,{"v":0.6279097374885,"d":"0.63"},{"$f":"VLOOKUP(A938,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.48468524699999993,"d":"0.48"}]
["01125","01","AL","125","Tuscaloosa","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2045.2456585383095,"A","CEC Survey",2017,15,"I",1284.2296645522842,"TON",8,{"v":0.6279097374885,"d":"0.63"},{"$f":"VLOOKUP(A939,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.48468524699999993,"d":"0.48"}]
["01125","01","AL","125","Tuscaloosa","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1396.7531326603091,"A","CEC Survey",2017,15,"I",877.0348928649747,"TON",8,{"v":0.6279097374885,"d":"0.63"},{"$f":"VLOOKUP(A940,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.48468524699999993,"d":"0.48"}]
["01125","01","AL","125","Tuscaloosa","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,8706.149652159476,"A","CEC Survey",2017,15,"I",1660.8315568479238,"TON",8,{"v":0.19076533521750003,"d":"0.19"},{"$f":"VLOOKUP(A941,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.147252285,"d":"0.15"}]
["01125","01","AL","125","Tuscaloosa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1724.8952860947795,"A","CEC Survey",2017,15,"I",386.44787540489176,"TON",8,{"v":0.224041354,"d":"0.22"},{"$f":"VLOOKUP(A942,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.17293813508297953,"d":"0.17"}]
["01125","01","AL","125","Tuscaloosa","","2104009000","Wax Log; Total: All Combustor Types",null,1027.0530512923356,"A","CEC Survey",2017,15,"I",240.4662931210925,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A943,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.180727363952142,"d":"0.18"}]
["01125","01","AL","125","Tuscaloosa","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1695.416495315962,"A","CEC Survey",2017,15,"I",1397.889217717841,"TON",8,{"v":0.8245108040295,"d":"0.82"},{"$f":"VLOOKUP(A944,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.636442149,"d":"0.64"}]
["01125","01","AL","125","Tuscaloosa","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2242.325042192079,"A","CEC Survey",2017,15,"I",1848.8212234332734,"TON",8,{"v":0.8245108040294999,"d":"0.82"},{"$f":"VLOOKUP(A945,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.636442149,"d":"0.64"}]
["01125","01","AL","125","Tuscaloosa","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1531.3439312531273,"A","CEC Survey",2017,15,"I",1262.6096160032114,"TON",8,{"v":0.8245108040295,"d":"0.82"},{"$f":"VLOOKUP(A946,cordwood_density!A:D,4,FALSE)","v":1.2955},{"v":0.636442149,"d":"0.64"}]
["01127","01","AL","127","Walker","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",144.1288523058038,"A","CEC Survey",2017,15,"I",247.8098422525294,"TON",8,{"v":1.7193631829298244,"d":"1.72"},{"$f":"VLOOKUP(A947,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":1.2597913122287694,"d":"1.26"}]
["01127","01","AL","127","Walker","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.686123159930037,"A","CEC Survey",2017,15,"I",20.09268991236725,"TON",8,{"v":1.7193631829298246,"d":"1.72"},{"$f":"VLOOKUP(A948,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":1.2597913122287694,"d":"1.26"}]
["01127","01","AL","127","Walker","","2104008610","Hydronic heater: outdoor","Hydronic heater",140.23347791916046,"A","CEC Survey",2017,15,"I",241.11227894840695,"TON",8,{"v":1.7193631829298242,"d":"1.72"},{"$f":"VLOOKUP(A949,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":1.2597913122287692,"d":"1.26"}]
["01127","01","AL","127","Walker","","2104008620","Hydronic heater: indoor","Hydronic heater",89.59361089279696,"A","CEC Survey",2017,15,"I",154.04395599481558,"TON",8,{"v":1.7193631829298246,"d":"1.72"},{"$f":"VLOOKUP(A950,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":1.2597913122287694,"d":"1.26"}]
["01127","01","AL","127","Walker","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.895374386643346,"A","CEC Survey",2017,15,"I",6.697563304122416,"TON",8,{"v":1.7193631829298244,"d":"1.72"},{"$f":"VLOOKUP(A951,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":1.2597913122287694,"d":"1.26"}]
["01127","01","AL","127","Walker","","2104008100","Fireplace: general","Fireplace: general",2518.7625304979997,"A","CEC Survey",2017,15,"I",693.6066449151714,"TON",8,{"v":0.2753759580416,"d":"0.28"},{"$f":"VLOOKUP(A952,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.201770192,"d":"0.20"}]
["01127","01","AL","127","Walker","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",773.4524651513101,"A","CEC Survey",2017,15,"I",464.2219122366179,"TON",8,{"v":0.6001944956575999,"d":"0.60"},{"$f":"VLOOKUP(A953,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.4397673619999999,"d":"0.44"}]
["01127","01","AL","127","Walker","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1022.95326036141,"A","CEC Survey",2017,15,"I",613.970916183914,"TON",8,{"v":0.6001944956576,"d":"0.60"},{"$f":"VLOOKUP(A954,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.439767362,"d":"0.44"}]
["01127","01","AL","127","Walker","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",698.6022265882801,"A","CEC Survey",2017,15,"I",419.29721105242913,"TON",8,{"v":0.6001944956576,"d":"0.60"},{"$f":"VLOOKUP(A955,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.439767362,"d":"0.44"}]
["01127","01","AL","127","Walker","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3707.2550181149995,"A","CEC Survey",2017,15,"I",746.5238314248008,"TON",8,{"v":0.201368351456,"d":"0.20"},{"$f":"VLOOKUP(A956,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.14754422,"d":"0.15"}]
["01127","01","AL","127","Walker","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",873.400889334,"A","CEC Survey",2017,15,"I",259.96394746756806,"TON",8,{"v":0.297645618,"d":"0.30"},{"$f":"VLOOKUP(A957,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.218087351992966,"d":"0.22"}]
["01127","01","AL","127","Walker","","2104009000","Wax Log; Total: All Combustor Types",null,210.70512861,"A","CEC Survey",2017,15,"I",72.36219893712153,"TON",8,{"v":0.34342874999999995,"d":"0.34"},{"$f":"VLOOKUP(A958,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.25163302315357555,"d":"0.25"}]
["01127","01","AL","127","Walker","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1042.38373279548,"A","CEC Survey",2017,15,"I",1075.3261448781275,"TON",8,{"v":1.0316029606432,"d":"1.03"},{"$f":"VLOOKUP(A959,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.755863834,"d":"0.76"}]
["01127","01","AL","127","Walker","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1378.6365498262799,"A","CEC Survey",2017,15,"I",1422.2055464517168,"TON",8,{"v":1.0316029606432,"d":"1.03"},{"$f":"VLOOKUP(A960,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.755863834,"d":"0.76"}]
["01127","01","AL","127","Walker","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",941.5078876862401,"A","CEC Survey",2017,15,"I",971.2623244060507,"TON",8,{"v":1.0316029606432,"d":"1.03"},{"$f":"VLOOKUP(A961,cordwood_density!A:D,4,FALSE)","v":1.3648},{"v":0.755863834,"d":"0.76"}]
["01129","01","AL","129","Washington","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",38.21648454032653,"A","CEC Survey",2017,15,"I",59.868416176848044,"TON",8,{"v":1.5665600040651073,"d":"1.57"},{"$f":"VLOOKUP(A962,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":1.216651137049633,"d":"1.22"}]
["01129","01","AL","129","Washington","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.098633881648097,"A","CEC Survey",2017,15,"I",4.854195906230922,"TON",8,{"$f":"P963/J963","v":{"v":1.5665600040651073,"d":"1.57"}},{"$f":"VLOOKUP(A963,cordwood_density!A:D,4,FALSE)","v":1.2876},{"$f":"S963/T963","v":{"v":1.216651137049633,"d":"1.22"}}]
["01129","01","AL","129","Washington","","2104008610","Hydronic heater: outdoor","Hydronic heater",37.18360657977717,"A","CEC Survey",2017,15,"I",58.25035087477107,"TON",8,{"v":1.5665600040651073,"d":"1.57"},{"$f":"VLOOKUP(A964,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":1.216651137049633,"d":"1.22"}]
["01129","01","AL","129","Washington","","2104008620","Hydronic heater: indoor","Hydronic heater",23.756193092635414,"A","CEC Survey",2017,15,"I",37.215501947770406,"TON",8,{"v":1.5665600040651073,"d":"1.57"},{"$f":"VLOOKUP(A965,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":1.216651137049633,"d":"1.22"}]
["01129","01","AL","129","Washington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0328779605493659,"A","CEC Survey",2017,15,"I",1.6180653020769742,"TON",8,{"v":1.566560004065107,"d":"1.57"},{"$f":"VLOOKUP(A966,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":1.2166511370496327,"d":"1.22"}]
["01129","01","AL","129","Washington","","2104008100","Fireplace: general","Fireplace: general",702.95263925,"A","CEC Survey",2017,15,"I",199.37036921205188,"TON",8,{"v":0.2836184944476,"d":"0.28"},{"$f":"VLOOKUP(A967,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.220269101,"d":"0.22"}]
["01129","01","AL","129","Washington","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",210.43228072242002,"A","CEC Survey",2017,15,"I",135.07856558166415,"TON",8,{"v":0.6419099062079999,"d":"0.64"},{"$f":"VLOOKUP(A968,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.49853207999999993,"d":"0.50"}]
["01129","01","AL","129","Washington","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",278.31366160062,"A","CEC Survey",2017,15,"I",178.65229641445904,"TON",8,{"v":0.641909906208,"d":"0.64"},{"$f":"VLOOKUP(A969,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.49853208,"d":"0.50"}]
["01129","01","AL","129","Washington","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",190.06786645896003,"A","CEC Survey",2017,15,"I",122.0064463318257,"TON",8,{"v":0.641909906208,"d":"0.64"},{"$f":"VLOOKUP(A970,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.49853208,"d":"0.50"}]
["01129","01","AL","129","Washington","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,993.979403628,"A","CEC Survey",2017,15,"I",189.35917894676697,"TON",8,{"v":0.1905061395192,"d":"0.19"},{"$f":"VLOOKUP(A971,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.147954442,"d":"0.15"}]
["01129","01","AL","129","Washington","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",249.148845888,"A","CEC Survey",2017,15,"I",68.921252197221,"TON",8,{"v":0.276626817,"d":"0.28"},{"$f":"VLOOKUP(A972,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.21483909366262816,"d":"0.21"}]
["01129","01","AL","129","Washington","","2104009000","Wax Log; Total: All Combustor Types",null,86.19219603209794,"A","CEC Survey",2017,15,"I",20.180377099045963,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A973,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.1818362068965517,"d":"0.18"}]
["01129","01","AL","129","Washington","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",279.28521125858003,"A","CEC Survey",2017,15,"I",284.05838604367375,"TON",8,{"v":1.0170906821868,"d":"1.02"},{"$f":"VLOOKUP(A974,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.7899119929999999,"d":"0.79"}]
["01129","01","AL","129","Washington","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",369.37721489038,"A","CEC Survey",2017,15,"I",375.69012347711686,"TON",8,{"v":1.0170906821868002,"d":"1.02"},{"$f":"VLOOKUP(A975,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.7899119930000001,"d":"0.79"}]
["01129","01","AL","129","Washington","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",252.25761016904002,"A","CEC Survey",2017,15,"I",256.5688648136408,"TON",8,{"v":1.0170906821868002,"d":"1.02"},{"$f":"VLOOKUP(A976,cordwood_density!A:D,4,FALSE)","v":1.2876},{"v":0.7899119930000001,"d":"0.79"}]
["01131","01","AL","131","Wilcox","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",20.405754119160576,"A","CEC Survey",2017,15,"I",32.964961281869606,"TON",8,{"v":1.6154738065238272,"d":"1.62"},{"$f":"VLOOKUP(A977,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":1.2437245411685482,"d":"1.24"}]
["01131","01","AL","131","Wilcox","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.6545206042562628,"A","CEC Survey",2017,15,"I",2.672834698529968,"TON",8,{"v":1.6154738065238274,"d":"1.62"},{"$f":"VLOOKUP(A978,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":1.2437245411685485,"d":"1.24"}]
["01131","01","AL","131","Wilcox","","2104008610","Hydronic heater: outdoor","Hydronic heater",19.854247251075154,"A","CEC Survey",2017,15,"I",32.074016382359616,"TON",8,{"v":1.6154738065238274,"d":"1.62"},{"$f":"VLOOKUP(A979,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":1.2437245411685485,"d":"1.24"}]
["01131","01","AL","131","Wilcox","","2104008620","Hydronic heater: indoor","Hydronic heater",12.684657965964684,"A","CEC Survey",2017,15,"I",20.491732688729755,"TON",8,{"v":1.6154738065238272,"d":"1.62"},{"$f":"VLOOKUP(A980,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":1.2437245411685482,"d":"1.24"}]
["01131","01","AL","131","Wilcox","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.551506868085421,"A","CEC Survey",2017,15,"I",0.8909448995099893,"TON",8,{"v":1.6154738065238272,"d":"1.62"},{"$f":"VLOOKUP(A981,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":1.2437245411685482,"d":"1.24"}]
["01131","01","AL","131","Wilcox","","2104008100","Fireplace: general","Fireplace: general",344.85907262899997,"A","CEC Survey",2017,15,"I",99.62529465957883,"TON",8,{"v":0.2888869760627,"d":"0.29"},{"$f":"VLOOKUP(A982,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.222408943,"d":"0.22"}]
["01131","01","AL","131","Wilcox","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",124.25573355791,"A","CEC Survey",2017,15,"I",72.09771407579615,"TON",8,{"v":0.5802365171518998,"d":"0.58"},{"$f":"VLOOKUP(A983,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.44671377099999987,"d":"0.45"}]
["01131","01","AL","131","Wilcox","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",164.33822825401,"A","CEC Survey",2017,15,"I",95.35504119702071,"TON",8,{"v":0.5802365171518998,"d":"0.58"},{"$f":"VLOOKUP(A984,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.44671377099999987,"d":"0.45"}]
["01131","01","AL","131","Wilcox","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",112.23098514908001,"A","CEC Survey",2017,15,"I",65.12051593942878,"TON",8,{"v":0.5802365171518998,"d":"0.58"},{"$f":"VLOOKUP(A985,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.44671377099999987,"d":"0.45"}]
["01131","01","AL","131","Wilcox","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,551.214477665,"A","CEC Survey",2017,15,"I",105.90412689994173,"TON",8,{"v":0.1921287106764,"d":"0.19"},{"$f":"VLOOKUP(A986,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.14791647600000002,"d":"0.15"}]
["01131","01","AL","131","Wilcox","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",136.82992111500002,"A","CEC Survey",2017,15,"I",36.65087078896983,"TON",8,{"v":0.267857136,"d":"0.27"},{"$f":"VLOOKUP(A987,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.20621844329817537,"d":"0.21"}]
["01131","01","AL","131","Wilcox","","2104009000","Wax Log; Total: All Combustor Types",null,55.16817613052628,"A","CEC Survey",2017,15,"I",12.916651964245217,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A988,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.18025429209330973,"d":"0.18"}]
["01131","01","AL","131","Wilcox","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",165.32881658456003,"A","CEC Survey",2017,15,"I",169.8644641926084,"TON",8,{"v":1.0274341019415,"d":"1.03"},{"$f":"VLOOKUP(A989,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.7910032350000001,"d":"0.79"}]
["01131","01","AL","131","Wilcox","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",218.66069290216,"A","CEC Survey",2017,15,"I",224.6594526418369,"TON",8,{"v":1.0274341019415,"d":"1.03"},{"$f":"VLOOKUP(A990,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.7910032350000001,"d":"0.79"}]
["01131","01","AL","131","Wilcox","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",149.32925368928002,"A","CEC Survey",2017,15,"I",153.42596765783986,"TON",8,{"v":1.0274341019415,"d":"1.03"},{"$f":"VLOOKUP(A991,cordwood_density!A:D,4,FALSE)","v":1.2989},{"v":0.7910032350000001,"d":"0.79"}]
["01133","01","AL","133","Winston","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",60.63382285124453,"A","CEC Survey",2017,15,"I",98.81465164549378,"TON",8,{"v":1.6296952261763185,"d":"1.63"},{"$f":"VLOOKUP(A992,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":1.2460396254884305,"d":"1.25"}]
["01133","01","AL","133","Winston","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.916255906857665,"A","CEC Survey",2017,15,"I",8.011998782067064,"TON",8,{"v":1.6296952261763185,"d":"1.63"},{"$f":"VLOOKUP(A993,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":1.2460396254884305,"d":"1.25"}]
["01133","01","AL","133","Winston","","2104008610","Hydronic heater: outdoor","Hydronic heater",58.99507088229198,"A","CEC Survey",2017,15,"I",96.14398538480475,"TON",8,{"v":1.6296952261763182,"d":"1.63"},{"$f":"VLOOKUP(A994,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":1.2460396254884305,"d":"1.25"}]
["01133","01","AL","133","Winston","","2104008620","Hydronic heater: indoor","Hydronic heater",37.691295285908765,"A","CEC Survey",2017,15,"I",61.425323995847485,"TON",8,{"v":1.6296952261763182,"d":"1.63"},{"$f":"VLOOKUP(A995,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":1.2460396254884305,"d":"1.25"}]
["01133","01","AL","133","Winston","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.638751968952555,"A","CEC Survey",2017,15,"I",2.6706662606890212,"TON",8,{"v":1.6296952261763185,"d":"1.63"},{"$f":"VLOOKUP(A996,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":1.2460396254884305,"d":"1.25"}]
["01133","01","AL","133","Winston","","2104008100","Fireplace: general","Fireplace: general",1034.1997509349999,"A","CEC Survey",2017,15,"I",283.5566455240119,"TON",8,{"v":0.2741797658215,"d":"0.27"},{"$f":"VLOOKUP(A997,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.20963358499999998,"d":"0.21"}]
["01133","01","AL","133","Winston","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",287.97124976315,"A","CEC Survey",2017,15,"I",170.99583269553636,"TON",8,{"v":0.5937948070725,"d":"0.59"},{"$f":"VLOOKUP(A998,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.45400627499999996,"d":"0.45"}]
["01133","01","AL","133","Winston","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",380.86520129965,"A","CEC Survey",2017,15,"I",226.15577872635455,"TON",8,{"v":0.5937948070725001,"d":"0.59"},{"$f":"VLOOKUP(A999,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.45400627500000007,"d":"0.45"}]
["01133","01","AL","133","Winston","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",260.10306430220004,"A","CEC Survey",2017,15,"I",154.44784888629093,"TON",8,{"v":0.5937948070725,"d":"0.59"},{"$f":"VLOOKUP(A1000,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.45400627499999996,"d":"0.45"}]
["01133","01","AL","133","Winston","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1466.020097288,"A","CEC Survey",2017,15,"I",282.7639960107519,"TON",8,{"v":0.19287866280540003,"d":"0.19"},{"$f":"VLOOKUP(A1001,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.147472026,"d":"0.15"}]
["01133","01","AL","133","Winston","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",359.92523900699996,"A","CEC Survey",2017,15,"I",106.09993135158498,"TON",8,{"v":0.294783249,"d":"0.29"},{"$f":"VLOOKUP(A1002,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.22538668782016974,"d":"0.23"}]
["01133","01","AL","133","Winston","","2104009000","Wax Log; Total: All Combustor Types",null,135.57209437543284,"A","CEC Survey",2017,15,"I",46.55935490623693,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1003,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.262580281367077,"d":"0.26"}]
["01133","01","AL","133","Winston","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",407.83533132287,"A","CEC Survey",2017,15,"I",412.76814005812054,"TON",8,{"v":1.0120950990667001,"d":"1.01"},{"$f":"VLOOKUP(A1004,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.7738321730000001,"d":"0.77"}]
["01133","01","AL","133","Winston","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",539.39511562057,"A","CEC Survey",2017,15,"I",545.9191529800949,"TON",8,{"v":1.0120950990667,"d":"1.01"},{"$f":"VLOOKUP(A1005,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.773832173,"d":"0.77"}]
["01133","01","AL","133","Winston","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",368.36739603356006,"A","CEC Survey",2017,15,"I",372.82283618152826,"TON",8,{"v":1.0120950990667,"d":"1.01"},{"$f":"VLOOKUP(A1006,cordwood_density!A:D,4,FALSE)","v":1.3079},{"v":0.773832173,"d":"0.77"}]
["02013","02","AK","013","Aleutians East","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1007,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1008,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1009,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1010,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1011,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104008100","Fireplace: general","Fireplace: general",0.468,"A","CEC Survey",2017,15,"I",0.00787644,"TON",8,{"v":0.016829999999999998,"d":"0.02"},{"$f":"VLOOKUP(A1012,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.016377968080965352,"d":"0.02"}]
["02013","02","AK","013","Aleutians East","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",7.2540000000000004,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1013,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02013","02","AK","013","Aleutians East","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",9.594,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1014,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02013","02","AK","013","Aleutians East","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",6.552000000000001,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1015,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02013","02","AK","013","Aleutians East","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1016,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1017,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1018,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02013","02","AK","013","Aleutians East","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",7.2540000000000004,"A","CEC Survey",2017,15,"I",6.104241000000001,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1019,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02013","02","AK","013","Aleutians East","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",9.594,"A","CEC Survey",2017,15,"I",8.073351,"TON",8,{"v":0.8415000000000001,"d":"0.84"},{"$f":"VLOOKUP(A1020,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482679,"d":"0.82"}]
["02013","02","AK","013","Aleutians East","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",6.552000000000001,"A","CEC Survey",2017,15,"I",5.513508000000001,"TON",8,{"v":0.8414999999999999,"d":"0.84"},{"$f":"VLOOKUP(A1021,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482676,"d":"0.82"}]
["02016","02","AK","016","Aleutians West","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1022,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1023,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1024,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1025,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1026,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104008100","Fireplace: general","Fireplace: general",1.078,"A","CEC Survey",2017,15,"I",1.4514192000000001,"TON",8,{"$f":"P1027/J1027","v":{"v":1.3464,"d":"1.35"}},{"$f":"VLOOKUP(A1027,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S1027/T1027","v":{"v":1.3102374464772284,"d":"1.31"}}]
["02016","02","AK","016","Aleutians West","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",16.709000000000003,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1028,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02016","02","AK","016","Aleutians West","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",22.099,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1029,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02016","02","AK","016","Aleutians West","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",15.092000000000002,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1030,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02016","02","AK","016","Aleutians West","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1031,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1032,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1033,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02016","02","AK","016","Aleutians West","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",50.126999999999995,"A","CEC Survey",2017,15,"I",210.9093525,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1034,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02016","02","AK","016","Aleutians West","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",66.297,"A","CEC Survey",2017,15,"I",278.94462749999997,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1035,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02016","02","AK","016","Aleutians West","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",45.276,"A","CEC Survey",2017,15,"I",190.49877000000004,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1036,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02020","02","AK","020","Anchorage","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1037,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02020","02","AK","020","Anchorage","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1038,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02020","02","AK","020","Anchorage","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1039,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02020","02","AK","020","Anchorage","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1040,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02020","02","AK","020","Anchorage","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1041,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02020","02","AK","020","Anchorage","","2104008100","Fireplace: general","Fireplace: general",16044.3,"A","CEC Survey",2017,15,"I",20251.917674999997,"TON",8,{"v":1.2622499999999999,"d":"1.26"},{"$f":"VLOOKUP(A1042,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724015,"d":"1.23"}]
["02020","02","AK","020","Anchorage","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",4973.733,"A","CEC Survey",2017,15,"I",16741.585278,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1043,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02020","02","AK","020","Anchorage","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6578.163,"A","CEC Survey",2017,15,"I",22142.096658,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1044,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02020","02","AK","020","Anchorage","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",4492.404,"A","CEC Survey",2017,15,"I",15121.431864000002,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1045,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02020","02","AK","020","Anchorage","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,18718.35,"A","CEC Survey",2017,15,"I",23627.2372875,"TON",8,{"v":1.26225,"d":"1.26"},{"$f":"VLOOKUP(A1046,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724017,"d":"1.23"}]
["02020","02","AK","020","Anchorage","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1604.4299999999998,"A","CEC Survey",2017,15,"I",401.10749999999996,"TON",8,0.25,{"$f":"VLOOKUP(A1047,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02020","02","AK","020","Anchorage","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1048,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02020","02","AK","020","Anchorage","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",9947.466,"A","CEC Survey",2017,15,"I",66966.341112,"TON",8,{"v":6.731999999999999,"d":"6.73"},{"$f":"VLOOKUP(A1049,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386141,"d":"6.55"}]
["02020","02","AK","020","Anchorage","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",13156.326,"A","CEC Survey",2017,15,"I",88568.386632,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1050,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02020","02","AK","020","Anchorage","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",8984.808,"A","CEC Survey",2017,15,"I",60485.72745600001,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1051,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02050","02","AK","050","Bethel","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1052,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02050","02","AK","050","Bethel","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1053,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02050","02","AK","050","Bethel","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1054,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02050","02","AK","050","Bethel","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1055,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02050","02","AK","050","Bethel","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1056,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02050","02","AK","050","Bethel","","2104008100","Fireplace: general","Fireplace: general",123.525,"A","CEC Survey",2017,15,"I",207.89257500000002,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1057,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02050","02","AK","050","Bethel","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",134.024625,"A","CEC Survey",2017,15,"I",563.9086096875,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1058,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02050","02","AK","050","Bethel","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",177.25837499999997,"A","CEC Survey",2017,15,"I",745.8146128125,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1059,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02050","02","AK","050","Bethel","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",121.0545,"A","CEC Survey",2017,15,"I",509.33680875000005,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1060,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02050","02","AK","050","Bethel","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,741.15,"A","CEC Survey",2017,15,"I",935.5165874999999,"TON",8,{"v":1.2622499999999999,"d":"1.26"},{"$f":"VLOOKUP(A1061,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724015,"d":"1.23"}]
["02050","02","AK","050","Bethel","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1062,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02050","02","AK","050","Bethel","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1063,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02050","02","AK","050","Bethel","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",153.171,"A","CEC Survey",2017,15,"I",644.4669825,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1064,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02050","02","AK","050","Bethel","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",202.581,"A","CEC Survey",2017,15,"I",852.3595574999999,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1065,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02050","02","AK","050","Bethel","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",138.348,"A","CEC Survey",2017,15,"I",582.09921,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1066,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02060","02","AK","060","Bristol Bay","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1067,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02060","02","AK","060","Bristol Bay","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1068,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02060","02","AK","060","Bristol Bay","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1069,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02060","02","AK","060","Bristol Bay","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1070,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02060","02","AK","060","Bristol Bay","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1071,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02060","02","AK","060","Bristol Bay","","2104008100","Fireplace: general","Fireplace: general",10.625,"A","CEC Survey",2017,15,"I",17.881875,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1072,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02060","02","AK","060","Bristol Bay","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",10.54,"A","CEC Survey",2017,15,"I",44.34705,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1073,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02060","02","AK","060","Bristol Bay","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",13.94,"A","CEC Survey",2017,15,"I",58.65255,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1074,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02060","02","AK","060","Bristol Bay","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",9.520000000000001,"A","CEC Survey",2017,15,"I",40.055400000000006,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1075,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02060","02","AK","060","Bristol Bay","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,106.25,"A","CEC Survey",2017,15,"I",134.11406250000002,"TON",8,{"v":1.26225,"d":"1.26"},{"$f":"VLOOKUP(A1076,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724017,"d":"1.23"}]
["02060","02","AK","060","Bristol Bay","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1077,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02060","02","AK","060","Bristol Bay","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1078,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02060","02","AK","060","Bristol Bay","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",52.7,"A","CEC Survey",2017,15,"I",221.73524999999998,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1079,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02060","02","AK","060","Bristol Bay","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",69.7,"A","CEC Survey",2017,15,"I",293.26275,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1080,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02060","02","AK","060","Bristol Bay","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",47.6,"A","CEC Survey",2017,15,"I",200.27700000000002,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1081,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02068","02","AK","068","Denali","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",5.32763,"A","CEC Survey",2017,15,"I",35.86560516,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1082,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02068","02","AK","068","Denali","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.43197,"A","CEC Survey",2017,15,"I",2.90802204,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1083,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02068","02","AK","068","Denali","","2104008610","Hydronic heater: outdoor","Hydronic heater",5.1836400000000005,"A","CEC Survey",2017,15,"I",34.89626448,"TON",8,{"v":6.731999999999999,"d":"6.73"},{"$f":"VLOOKUP(A1084,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386141,"d":"6.55"}]
["02068","02","AK","068","Denali","","2104008620","Hydronic heater: indoor","Hydronic heater",3.3117700000000005,"A","CEC Survey",2017,15,"I",22.294835640000002,"TON",8,{"v":6.731999999999999,"d":"6.73"},{"$f":"VLOOKUP(A1085,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386141,"d":"6.55"}]
["02068","02","AK","068","Denali","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.14399,"A","CEC Survey",2017,15,"I",0.9693406800000002,"TON",8,{"v":6.732000000000001,"d":"6.73"},{"$f":"VLOOKUP(A1086,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386143,"d":"6.55"}]
["02068","02","AK","068","Denali","","2104008100","Fireplace: general","Fireplace: general",42.35,"A","CEC Survey",2017,15,"I",213.82515000000004,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1087,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02068","02","AK","068","Denali","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",13.1285,"A","CEC Survey",2017,15,"I",77.33342925,"TON",8,{"v":5.890499999999999,"d":"5.89"},{"$f":"VLOOKUP(A1088,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.7322888283378735,"d":"5.73"}]
["02068","02","AK","068","Denali","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",17.3635,"A","CEC Survey",2017,15,"I",102.27969674999999,"TON",8,{"v":5.890499999999999,"d":"5.89"},{"$f":"VLOOKUP(A1089,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.7322888283378735,"d":"5.73"}]
["02068","02","AK","068","Denali","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",11.858000000000002,"A","CEC Survey",2017,15,"I",69.84954900000001,"TON",8,{"v":5.890499999999999,"d":"5.89"},{"$f":"VLOOKUP(A1090,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.7322888283378735,"d":"5.73"}]
["02068","02","AK","068","Denali","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,186.34,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$f":"P1091/J1091","v":{"v":0,"d":"0.00"}},{"$f":"VLOOKUP(A1091,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S1091/T1091","v":{"v":0,"d":"0.00"}}]
["02068","02","AK","068","Denali","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",16.94,"A","CEC Survey",2017,15,"I",4.235,"TON",8,0.25,{"$f":"VLOOKUP(A1092,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02068","02","AK","068","Denali","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1093,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02068","02","AK","068","Denali","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",65.6425,"A","CEC Survey",2017,15,"I",331.42898249999996,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1094,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02068","02","AK","068","Denali","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",86.8175,"A","CEC Survey",2017,15,"I",438.34155749999996,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1095,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02068","02","AK","068","Denali","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",59.290000000000006,"A","CEC Survey",2017,15,"I",299.35521,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1096,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02070","02","AK","070","Dillingham","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1097,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02070","02","AK","070","Dillingham","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1098,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02070","02","AK","070","Dillingham","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1099,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02070","02","AK","070","Dillingham","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1100,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02070","02","AK","070","Dillingham","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1101,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02070","02","AK","070","Dillingham","","2104008100","Fireplace: general","Fireplace: general",40.625,"A","CEC Survey",2017,15,"I",68.371875,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1102,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02070","02","AK","070","Dillingham","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",40.3,"A","CEC Survey",2017,15,"I",169.56225,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1103,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02070","02","AK","070","Dillingham","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",53.3,"A","CEC Survey",2017,15,"I",224.25975,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1104,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02070","02","AK","070","Dillingham","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",36.400000000000006,"A","CEC Survey",2017,15,"I",153.15300000000002,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1105,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02070","02","AK","070","Dillingham","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,406.25,"A","CEC Survey",2017,15,"I",512.7890625,"TON",8,{"v":1.26225,"d":"1.26"},{"$f":"VLOOKUP(A1106,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724017,"d":"1.23"}]
["02070","02","AK","070","Dillingham","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1107,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02070","02","AK","070","Dillingham","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1108,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02070","02","AK","070","Dillingham","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",201.5,"A","CEC Survey",2017,15,"I",847.81125,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1109,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02070","02","AK","070","Dillingham","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",266.5,"A","CEC Survey",2017,15,"I",1121.29875,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1110,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02070","02","AK","070","Dillingham","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",182.00000000000003,"A","CEC Survey",2017,15,"I",765.7650000000001,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1111,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02090","02","AK","090","Fairbanks North Star","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",399.4224,"A","CEC Survey",2017,15,"I",2688.9115967999996,"TON",8,{"v":6.731999999999999,"d":"6.73"},{"$f":"VLOOKUP(A1112,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.972320794889993,"d":"5.97"}]
["02090","02","AK","090","Fairbanks North Star","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",32.3856,"A","CEC Survey",2017,15,"I",218.01985919999998,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1113,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.972320794889993,"d":"5.97"}]
["02090","02","AK","090","Fairbanks North Star","","2104008610","Hydronic heater: outdoor","Hydronic heater",388.62719999999996,"A","CEC Survey",2017,15,"I",2616.2383103999996,"TON",8,{"v":6.731999999999999,"d":"6.73"},{"$f":"VLOOKUP(A1114,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.972320794889993,"d":"5.97"}]
["02090","02","AK","090","Fairbanks North Star","","2104008620","Hydronic heater: indoor","Hydronic heater",248.2896,"A","CEC Survey",2017,15,"I",1671.4855872,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1115,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.972320794889993,"d":"5.97"}]
["02090","02","AK","090","Fairbanks North Star","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.7952,"A","CEC Survey",2017,15,"I",72.6732864,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1116,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.972320794889993,"d":"5.97"}]
["02090","02","AK","090","Fairbanks North Star","","2104008100","Fireplace: general","Fireplace: general",2518.88,"A","CEC Survey",2017,15,"I",12717.825120000001,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1117,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":4.479240596167495,"d":"4.48"}]
["02090","02","AK","090","Fairbanks North Star","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",355.52191999999997,"A","CEC Survey",2017,15,"I",2094.20186976,"TON",8,{"v":5.890500000000001,"d":"5.89"},{"$f":"VLOOKUP(A1118,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.225780695528745,"d":"5.23"}]
["02090","02","AK","090","Fairbanks North Star","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1085.2774399999998,"A","CEC Survey",2017,15,"I",6392.82676032,"TON",8,{"v":5.890500000000001,"d":"5.89"},{"$f":"VLOOKUP(A1119,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.225780695528745,"d":"5.23"}]
["02090","02","AK","090","Fairbanks North Star","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",785.8905599999999,"A","CEC Survey",2017,15,"I",4629.28834368,"TON",8,{"v":5.890500000000001,"d":"5.89"},{"$f":"VLOOKUP(A1120,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":5.225780695528745,"d":"5.23"}]
["02090","02","AK","090","Fairbanks North Star","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1079.52,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1121,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":0,"d":"0.00"}]
["02090","02","AK","090","Fairbanks North Star","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",29866.719999999998,"A","CEC Survey",2017,15,"I",7466.679999999999,"TON",8,0.25,{"$f":"VLOOKUP(A1122,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":0.22178850248403123,"d":"0.22"}]
["02090","02","AK","090","Fairbanks North Star","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1123,cordwood_density!A:D,4,FALSE)","v":1.1272},{"$error":"#DIV/0!"}]
["02090","02","AK","090","Fairbanks North Star","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",4444.024,"A","CEC Survey",2017,15,"I",22437.877176,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1124,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":4.479240596167495,"d":"4.48"}]
["02090","02","AK","090","Fairbanks North Star","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",13565.968,"A","CEC Survey",2017,15,"I",68494.572432,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1125,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":4.479240596167494,"d":"4.48"}]
["02090","02","AK","090","Fairbanks North Star","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",9823.632000000001,"A","CEC Survey",2017,15,"I",49599.51796800001,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1126,cordwood_density!A:D,4,FALSE)","v":1.1272},{"v":4.479240596167495,"d":"4.48"}]
["02100","02","AK","100","Haines","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",33.230325,"A","CEC Survey",2017,15,"I",111.85327395,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1127,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02100","02","AK","100","Haines","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.69577,"A","CEC Survey",2017,15,"I",9.07396182,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1128,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02100","02","AK","100","Haines","","2104008610","Hydronic heater: outdoor","Hydronic heater",0.87525,"A","CEC Survey",2017,15,"I",2.9460915,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1129,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02100","02","AK","100","Haines","","2104008620","Hydronic heater: indoor","Hydronic heater",20.6559,"A","CEC Survey",2017,15,"I",69.5277594,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1130,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02100","02","AK","100","Haines","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.89859,"A","CEC Survey",2017,15,"I",3.0246539400000003,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1131,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02100","02","AK","100","Haines","","2104008100","Fireplace: general","Fireplace: general",58.35,"A","CEC Survey",2017,15,"I",49.101525,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1132,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02100","02","AK","100","Haines","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1133,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02100","02","AK","100","Haines","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1134,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02100","02","AK","100","Haines","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1135,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02100","02","AK","100","Haines","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,291.75,"A","CEC Survey",2017,15,"I",294.60915,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1136,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02100","02","AK","100","Haines","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",93.36,"A","CEC Survey",2017,15,"I",23.34,"TON",8,0.25,{"$f":"VLOOKUP(A1137,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02100","02","AK","100","Haines","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1138,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02100","02","AK","100","Haines","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",144.708,"A","CEC Survey",2017,15,"I",852.402474,"TON",8,{"v":5.8905,"d":"5.89"},{"$f":"VLOOKUP(A1139,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.732288828337874,"d":"5.73"}]
["02100","02","AK","100","Haines","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",191.388,"A","CEC Survey",2017,15,"I",1127.3710139999998,"TON",8,{"v":5.890499999999999,"d":"5.89"},{"$f":"VLOOKUP(A1140,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.7322888283378735,"d":"5.73"}]
["02100","02","AK","100","Haines","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",130.704,"A","CEC Survey",2017,15,"I",769.911912,"TON",8,{"v":5.8905,"d":"5.89"},{"$f":"VLOOKUP(A1141,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.732288828337874,"d":"5.73"}]
["02105","02","AK","105","Hoonah Angoon","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",3.4743000000000004,"A","CEC Survey",2017,15,"I",11.6944938,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1142,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02105","02","AK","105","Hoonah Angoon","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.2817,"A","CEC Survey",2017,15,"I",0.9482022,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1143,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02105","02","AK","105","Hoonah Angoon","","2104008610","Hydronic heater: outdoor","Hydronic heater",3.3804000000000003,"A","CEC Survey",2017,15,"I",11.3784264,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1144,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02105","02","AK","105","Hoonah Angoon","","2104008620","Hydronic heater: indoor","Hydronic heater",2.1597000000000004,"A","CEC Survey",2017,15,"I",7.269550200000001,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1145,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02105","02","AK","105","Hoonah Angoon","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.09390000000000001,"A","CEC Survey",2017,15,"I",0.31606740000000005,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1146,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02105","02","AK","105","Hoonah Angoon","","2104008100","Fireplace: general","Fireplace: general",46.95,"A","CEC Survey",2017,15,"I",39.508425,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1147,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02105","02","AK","105","Hoonah Angoon","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",14.5545,"A","CEC Survey",2017,15,"I",24.4952235,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1148,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02105","02","AK","105","Hoonah Angoon","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",19.2495,"A","CEC Survey",2017,15,"I",32.3969085,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1149,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02105","02","AK","105","Hoonah Angoon","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",13.146000000000003,"A","CEC Survey",2017,15,"I",22.124718000000005,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1150,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02105","02","AK","105","Hoonah Angoon","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,140.85,"A","CEC Survey",2017,15,"I",142.23032999999998,"TON",8,{"v":1.0097999999999998,"d":"1.01"},{"$f":"VLOOKUP(A1151,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579211,"d":"0.98"}]
["02105","02","AK","105","Hoonah Angoon","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",80.75399999999999,"A","CEC Survey",2017,15,"I",20.188499999999998,"TON",8,0.25,{"$f":"VLOOKUP(A1152,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02105","02","AK","105","Hoonah Angoon","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1153,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02105","02","AK","105","Hoonah Angoon","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",101.88149999999999,"A","CEC Survey",2017,15,"I",342.93312899999995,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1154,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02105","02","AK","105","Hoonah Angoon","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",134.74649999999997,"A","CEC Survey",2017,15,"I",453.55671899999993,"TON",8,{"$f":"P1155/J1155","v":{"v":3.366,"d":"3.37"}},{"$f":"VLOOKUP(A1155,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S1155/T1155","v":{"v":3.275593616193071,"d":"3.28"}}]
["02105","02","AK","105","Hoonah Angoon","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",92.022,"A","CEC Survey",2017,15,"I",309.746052,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1156,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",45.0179,"A","CEC Survey",2017,15,"I",151.5302514,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1157,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.6501,"A","CEC Survey",2017,15,"I",12.2862366,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1158,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008610","Hydronic heater: outdoor","Hydronic heater",43.8012,"A","CEC Survey",2017,15,"I",147.4348392,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1159,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008620","Hydronic heater: indoor","Hydronic heater",27.9841,"A","CEC Survey",2017,15,"I",94.1944806,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1160,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2167000000000001,"A","CEC Survey",2017,15,"I",4.0954122,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1161,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008100","Fireplace: general","Fireplace: general",608.35,"A","CEC Survey",2017,15,"I",511.926525,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1162,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02110","02","AK","110","Juneau","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",188.5885,"A","CEC Survey",2017,15,"I",317.3944455,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1163,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02110","02","AK","110","Juneau","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",249.4235,"A","CEC Survey",2017,15,"I",419.7797505,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1164,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02110","02","AK","110","Juneau","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",170.33800000000002,"A","CEC Survey",2017,15,"I",286.67885400000006,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1165,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02110","02","AK","110","Juneau","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,669.1850000000001,"A","CEC Survey",2017,15,"I",675.743013,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1166,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02110","02","AK","110","Juneau","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",912.525,"A","CEC Survey",2017,15,"I",228.13125,"TON",8,0.25,{"$f":"VLOOKUP(A1167,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02110","02","AK","110","Juneau","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1168,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02110","02","AK","110","Juneau","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1131.531,"A","CEC Survey",2017,15,"I",3808.733346,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1169,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1496.541,"A","CEC Survey",2017,15,"I",5037.357006,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1170,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02110","02","AK","110","Juneau","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1022.028,"A","CEC Survey",2017,15,"I",3440.1462480000005,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1171,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02122","02","AK","122","Kenai Peninsula","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",421.8185,"A","CEC Survey",2017,15,"I",2129.7616064999997,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1172,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02122","02","AK","122","Kenai Peninsula","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",34.201499999999996,"A","CEC Survey",2017,15,"I",172.6833735,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1173,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02122","02","AK","122","Kenai Peninsula","","2104008610","Hydronic heater: outdoor","Hydronic heater",410.41799999999995,"A","CEC Survey",2017,15,"I",2072.2004819999997,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1174,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02122","02","AK","122","Kenai Peninsula","","2104008620","Hydronic heater: indoor","Hydronic heater",262.2115,"A","CEC Survey",2017,15,"I",1323.9058635,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1175,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02122","02","AK","122","Kenai Peninsula","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",11.4005,"A","CEC Survey",2017,15,"I",57.5611245,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1176,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02122","02","AK","122","Kenai Peninsula","","2104008100","Fireplace: general","Fireplace: general",3420.15,"A","CEC Survey",2017,15,"I",2878.0562250000003,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1177,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02122","02","AK","122","Kenai Peninsula","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",706.831,"A","CEC Survey",2017,15,"I",237.9193146,"TON",8,{"v":0.3366,"d":"0.34"},{"$f":"VLOOKUP(A1178,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3275593616193071,"d":"0.33"}]
["02122","02","AK","122","Kenai Peninsula","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",934.8409999999999,"A","CEC Survey",2017,15,"I",314.6674806,"TON",8,{"v":0.3366,"d":"0.34"},{"$f":"VLOOKUP(A1179,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3275593616193071,"d":"0.33"}]
["02122","02","AK","122","Kenai Peninsula","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",638.428,"A","CEC Survey",2017,15,"I",214.89486480000002,"TON",8,{"v":0.3366,"d":"0.34"},{"$f":"VLOOKUP(A1180,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3275593616193071,"d":"0.33"}]
["02122","02","AK","122","Kenai Peninsula","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2280.1,"A","CEC Survey",2017,15,"I",1918.70415,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1181,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02122","02","AK","122","Kenai Peninsula","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1140.05,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1182,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02122","02","AK","122","Kenai Peninsula","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1183,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02122","02","AK","122","Kenai Peninsula","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",4947.817,"A","CEC Survey",2017,15,"I",31226.910041249997,"TON",8,{"v":6.311249999999999,"d":"6.31"},{"$f":"VLOOKUP(A1184,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.141738030362007,"d":"6.14"}]
["02122","02","AK","122","Kenai Peninsula","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6543.886999999999,"A","CEC Survey",2017,15,"I",41300.106828749995,"TON",8,{"v":6.31125,"d":"6.31"},{"$f":"VLOOKUP(A1185,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.141738030362008,"d":"6.14"}]
["02122","02","AK","122","Kenai Peninsula","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",4468.996,"A","CEC Survey",2017,15,"I",28204.951005,"TON",8,{"v":6.311249999999999,"d":"6.31"},{"$f":"VLOOKUP(A1186,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.141738030362007,"d":"6.14"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",96.9585,"A","CEC Survey",2017,15,"I",326.36231100000003,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1187,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.8615,"A","CEC Survey",2017,15,"I",26.461809000000002,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1188,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008610","Hydronic heater: outdoor","Hydronic heater",94.338,"A","CEC Survey",2017,15,"I",317.541708,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1189,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008620","Hydronic heater: indoor","Hydronic heater",60.2715,"A","CEC Survey",2017,15,"I",202.87386900000004,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1190,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.6205000000000003,"A","CEC Survey",2017,15,"I",8.820603000000002,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1191,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008100","Fireplace: general","Fireplace: general",1048.2,"A","CEC Survey",2017,15,"I",882.0603000000001,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1192,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",81.2355,"A","CEC Survey",2017,15,"I",136.7193465,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1193,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",107.4405,"A","CEC Survey",2017,15,"I",180.8223615,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1194,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",73.37400000000001,"A","CEC Survey",2017,15,"I",123.48844200000002,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1195,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,786.15,"A","CEC Survey",2017,15,"I",793.8542699999999,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1196,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",393.075,"A","CEC Survey",2017,15,"I",98.26875,"TON",8,0.25,{"$f":"VLOOKUP(A1197,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02130","02","AK","130","Ketchikan Gateway","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1198,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",568.6485,"A","CEC Survey",2017,15,"I",3349.62398925,"TON",8,{"v":5.890499999999999,"d":"5.89"},{"$f":"VLOOKUP(A1199,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.7322888283378735,"d":"5.73"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",752.0835,"A","CEC Survey",2017,15,"I",4430.147856749999,"TON",8,{"v":5.8904999999999985,"d":"5.89"},{"$f":"VLOOKUP(A1200,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.732288828337873,"d":"5.73"}]
["02130","02","AK","130","Ketchikan Gateway","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",513.618,"A","CEC Survey",2017,15,"I",3025.466829,"TON",8,{"v":5.890499999999999,"d":"5.89"},{"$f":"VLOOKUP(A1201,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.7322888283378735,"d":"5.73"}]
["02150","02","AK","150","Kodiak Island","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",81.2335,"A","CEC Survey",2017,15,"I",410.14794150000006,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1202,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02150","02","AK","150","Kodiak Island","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.5865,"A","CEC Survey",2017,15,"I",33.255238500000004,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1203,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02150","02","AK","150","Kodiak Island","","2104008610","Hydronic heater: outdoor","Hydronic heater",79.038,"A","CEC Survey",2017,15,"I",399.06286200000005,"TON",8,{"v":5.049000000000001,"d":"5.05"},{"$f":"VLOOKUP(A1204,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289608,"d":"4.91"}]
["02150","02","AK","150","Kodiak Island","","2104008620","Hydronic heater: indoor","Hydronic heater",50.496500000000005,"A","CEC Survey",2017,15,"I",254.95682850000006,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1205,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02150","02","AK","150","Kodiak Island","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.1955,"A","CEC Survey",2017,15,"I",11.085079500000003,"TON",8,{"v":5.049000000000001,"d":"5.05"},{"$f":"VLOOKUP(A1206,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289608,"d":"4.91"}]
["02150","02","AK","150","Kodiak Island","","2104008100","Fireplace: general","Fireplace: general",658.65,"A","CEC Survey",2017,15,"I",554.253975,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1207,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02150","02","AK","150","Kodiak Island","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",136.121,"A","CEC Survey",2017,15,"I",45.8183286,"TON",8,{"v":0.3366,"d":"0.34"},{"$f":"VLOOKUP(A1208,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3275593616193071,"d":"0.33"}]
["02150","02","AK","150","Kodiak Island","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",180.031,"A","CEC Survey",2017,15,"I",60.5984346,"TON",8,{"v":0.33659999999999995,"d":"0.34"},{"$f":"VLOOKUP(A1209,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.32755936161930704,"d":"0.33"}]
["02150","02","AK","150","Kodiak Island","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",122.94800000000002,"A","CEC Survey",2017,15,"I",41.38429680000001,"TON",8,{"v":0.3366,"d":"0.34"},{"$f":"VLOOKUP(A1210,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3275593616193071,"d":"0.33"}]
["02150","02","AK","150","Kodiak Island","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1097.75,"A","CEC Survey",2017,15,"I",923.756625,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1211,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02150","02","AK","150","Kodiak Island","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",43.910000000000004,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1212,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02150","02","AK","150","Kodiak Island","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1213,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02150","02","AK","150","Kodiak Island","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",136.121,"A","CEC Survey",2017,15,"I",859.09366125,"TON",8,{"v":6.311249999999999,"d":"6.31"},{"$f":"VLOOKUP(A1214,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.141738030362007,"d":"6.14"}]
["02150","02","AK","150","Kodiak Island","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",180.031,"A","CEC Survey",2017,15,"I",1136.22064875,"TON",8,{"v":6.31125,"d":"6.31"},{"$f":"VLOOKUP(A1215,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.141738030362008,"d":"6.14"}]
["02150","02","AK","150","Kodiak Island","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",122.94800000000002,"A","CEC Survey",2017,15,"I",775.9555650000001,"TON",8,{"v":6.311249999999999,"d":"6.31"},{"$f":"VLOOKUP(A1216,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.141738030362007,"d":"6.14"}]
["02158","02","AK","158","Kusilvak","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1217,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02158","02","AK","158","Kusilvak","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1218,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02158","02","AK","158","Kusilvak","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$f":"P1219/J1219","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A1219,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S1219/T1219","v":{"$error":"#DIV/0!"}}]
["02158","02","AK","158","Kusilvak","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1220,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02158","02","AK","158","Kusilvak","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1221,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02158","02","AK","158","Kusilvak","","2104008100","Fireplace: general","Fireplace: general",97.85000000000001,"A","CEC Survey",2017,15,"I",164.68155000000002,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1222,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02158","02","AK","158","Kusilvak","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",30.3335,"A","CEC Survey",2017,15,"I",127.62820125000002,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1223,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02158","02","AK","158","Kusilvak","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",40.118500000000004,"A","CEC Survey",2017,15,"I",168.79858875,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1224,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02158","02","AK","158","Kusilvak","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",27.398000000000003,"A","CEC Survey",2017,15,"I",115.27708500000003,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1225,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02158","02","AK","158","Kusilvak","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,489.25,"A","CEC Survey",2017,15,"I",494.04465000000005,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1226,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02158","02","AK","158","Kusilvak","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1227,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02158","02","AK","158","Kusilvak","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1228,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02158","02","AK","158","Kusilvak","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",218.4012,"A","CEC Survey",2017,15,"I",918.923049,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1229,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02158","02","AK","158","Kusilvak","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",288.85319999999996,"A","CEC Survey",2017,15,"I",1215.3498389999997,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1230,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02158","02","AK","158","Kusilvak","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",197.2656,"A","CEC Survey",2017,15,"I",829.995012,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1231,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02164","02","AK","164","Lake and Peninsula","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1232,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02164","02","AK","164","Lake and Peninsula","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1233,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02164","02","AK","164","Lake and Peninsula","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1234,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02164","02","AK","164","Lake and Peninsula","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1235,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02164","02","AK","164","Lake and Peninsula","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1236,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02164","02","AK","164","Lake and Peninsula","","2104008100","Fireplace: general","Fireplace: general",29.05,"A","CEC Survey",2017,15,"I",48.89115,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1237,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02164","02","AK","164","Lake and Peninsula","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",0.5810000000000001,"A","CEC Survey",2017,15,"I",2.4445575,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1238,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02164","02","AK","164","Lake and Peninsula","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",13.943999999999999,"A","CEC Survey",2017,15,"I",58.66938,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1239,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02164","02","AK","164","Lake and Peninsula","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",43.575,"A","CEC Survey",2017,15,"I",183.3418125,"TON",8,{"v":4.2075,"d":"4.21"},{"$f":"VLOOKUP(A1240,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241338,"d":"4.09"}]
["02164","02","AK","164","Lake and Peninsula","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,145.25,"A","CEC Survey",2017,15,"I",183.3418125,"TON",8,{"v":1.26225,"d":"1.26"},{"$f":"VLOOKUP(A1241,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724017,"d":"1.23"}]
["02164","02","AK","164","Lake and Peninsula","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1242,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02164","02","AK","164","Lake and Peninsula","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1243,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02164","02","AK","164","Lake and Peninsula","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",5.229,"A","CEC Survey",2017,15,"I",22.001017500000003,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1244,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02164","02","AK","164","Lake and Peninsula","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",125.496,"A","CEC Survey",2017,15,"I",528.0244200000001,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1245,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02164","02","AK","164","Lake and Peninsula","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",392.17499999999995,"A","CEC Survey",2017,15,"I",1650.0763125000003,"TON",8,{"v":4.207500000000001,"d":"4.21"},{"$f":"VLOOKUP(A1246,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.09449202024134,"d":"4.09"}]
["02170","02","AK","170","Matanuska Susitna","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",197.1582,"A","CEC Survey",2017,15,"I",995.4517518,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1247,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02170","02","AK","170","Matanuska Susitna","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",15.9858,"A","CEC Survey",2017,15,"I",80.71230419999999,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1248,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02170","02","AK","170","Matanuska Susitna","","2104008610","Hydronic heater: outdoor","Hydronic heater",191.8296,"A","CEC Survey",2017,15,"I",968.5476504,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1249,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02170","02","AK","170","Matanuska Susitna","","2104008620","Hydronic heater: indoor","Hydronic heater",122.55780000000001,"A","CEC Survey",2017,15,"I",618.7943322,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1250,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02170","02","AK","170","Matanuska Susitna","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.328600000000001,"A","CEC Survey",2017,15,"I",26.904101400000002,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1251,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02170","02","AK","170","Matanuska Susitna","","2104008100","Fireplace: general","Fireplace: general",888.1,"A","CEC Survey",2017,15,"I",1121.0042250000001,"TON",8,{"v":1.26225,"d":"1.26"},{"$f":"VLOOKUP(A1252,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724017,"d":"1.23"}]
["02170","02","AK","170","Matanuska Susitna","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1156.3062,"A","CEC Survey",2017,15,"I",3892.1266692,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1253,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02170","02","AK","170","Matanuska Susitna","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1529.3082,"A","CEC Survey",2017,15,"I",5147.6514012,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1254,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02170","02","AK","170","Matanuska Susitna","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1044.4056,"A","CEC Survey",2017,15,"I",3515.4692496000002,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1255,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02170","02","AK","170","Matanuska Susitna","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,7104.8,"A","CEC Survey",2017,15,"I",8968.033800000001,"TON",8,{"v":1.26225,"d":"1.26"},{"$f":"VLOOKUP(A1256,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2283476060724017,"d":"1.23"}]
["02170","02","AK","170","Matanuska Susitna","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",603.908,"A","CEC Survey",2017,15,"I",150.977,"TON",8,0.25,{"$f":"VLOOKUP(A1257,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02170","02","AK","170","Matanuska Susitna","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1258,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02170","02","AK","170","Matanuska Susitna","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1651.8659999999998,"A","CEC Survey",2017,15,"I",11120.361911999998,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1259,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02170","02","AK","170","Matanuska Susitna","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2184.7259999999997,"A","CEC Survey",2017,15,"I",14707.575431999998,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1260,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02170","02","AK","170","Matanuska Susitna","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1492.008,"A","CEC Survey",2017,15,"I",10044.197856,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1261,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02180","02","AK","180","Nome","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1262,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02180","02","AK","180","Nome","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1263,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02180","02","AK","180","Nome","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1264,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02180","02","AK","180","Nome","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1265,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02180","02","AK","180","Nome","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1266,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02180","02","AK","180","Nome","","2104008100","Fireplace: general","Fireplace: general",73.625,"A","CEC Survey",2017,15,"I",61.9554375,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1267,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02180","02","AK","180","Nome","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",91.295,"A","CEC Survey",2017,15,"I",384.1237125,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1268,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02180","02","AK","180","Nome","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",120.74499999999999,"A","CEC Survey",2017,15,"I",508.0345875,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1269,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02180","02","AK","180","Nome","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",82.46000000000001,"A","CEC Survey",2017,15,"I",346.95045000000005,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1270,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02180","02","AK","180","Nome","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,294.5,"A","CEC Survey",2017,15,"I",297.3861,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1271,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02180","02","AK","180","Nome","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1272,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02180","02","AK","180","Nome","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1273,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02180","02","AK","180","Nome","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",91.295,"A","CEC Survey",2017,15,"I",384.1237125,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1274,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02180","02","AK","180","Nome","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",120.74499999999999,"A","CEC Survey",2017,15,"I",508.0345875,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1275,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02180","02","AK","180","Nome","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",82.46000000000001,"A","CEC Survey",2017,15,"I",346.95045000000005,"TON",8,{"v":4.2075000000000005,"d":"4.21"},{"$f":"VLOOKUP(A1276,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.094492020241339,"d":"4.09"}]
["02185","02","AK","185","North Slope","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1277,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1278,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1279,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1280,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1281,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008100","Fireplace: general","Fireplace: general",50.35,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1282,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02185","02","AK","185","North Slope","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$f":"P1283/J1283","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A1283,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S1283/T1283","v":{"$error":"#DIV/0!"}}]
["02185","02","AK","185","North Slope","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1284,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1285,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,201.4,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1286,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02185","02","AK","185","North Slope","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1287,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1288,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02185","02","AK","185","North Slope","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",62.434000000000005,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1289,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02185","02","AK","185","North Slope","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",82.574,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1290,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02185","02","AK","185","North Slope","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",56.39200000000001,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1291,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02188","02","AK","188","Northwest Arctic","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1292,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1293,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1294,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1295,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1296,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008100","Fireplace: general","Fireplace: general",98.95,"A","CEC Survey",2017,15,"I",83.266425,"TON",8,{"v":0.8414999999999999,"d":"0.84"},{"$f":"VLOOKUP(A1297,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482676,"d":"0.82"}]
["02188","02","AK","188","Northwest Arctic","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1298,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1299,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1300,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1301,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1302,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1303,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02188","02","AK","188","Northwest Arctic","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",306.745,"A","CEC Survey",2017,15,"I",2065.00734,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1304,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02188","02","AK","188","Northwest Arctic","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",405.695,"A","CEC Survey",2017,15,"I",2731.13874,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1305,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02188","02","AK","188","Northwest Arctic","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",277.06,"A","CEC Survey",2017,15,"I",1865.1679200000003,"TON",8,{"v":6.732000000000001,"d":"6.73"},{"$f":"VLOOKUP(A1306,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386143,"d":"6.55"}]
["02195","02","AK","195","Petersburg","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",24.753,"A","CEC Survey",2017,15,"I",83.31859800000001,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1307,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02195","02","AK","195","Petersburg","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.007,"A","CEC Survey",2017,15,"I",6.755562,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1308,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02195","02","AK","195","Petersburg","","2104008610","Hydronic heater: outdoor","Hydronic heater",24.084,"A","CEC Survey",2017,15,"I",81.066744,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1309,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02195","02","AK","195","Petersburg","","2104008620","Hydronic heater: indoor","Hydronic heater",15.387000000000002,"A","CEC Survey",2017,15,"I",51.79264200000001,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1310,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02195","02","AK","195","Petersburg","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.669,"A","CEC Survey",2017,15,"I",2.2518540000000002,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1311,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02195","02","AK","195","Petersburg","","2104008100","Fireplace: general","Fireplace: general",267.6,"A","CEC Survey",2017,15,"I",225.18540000000002,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1312,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02195","02","AK","195","Petersburg","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",20.739,"A","CEC Survey",2017,15,"I",34.903737,"TON",8,{"v":1.6829999999999998,"d":"1.68"},{"$f":"VLOOKUP(A1313,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965353,"d":"1.64"}]
["02195","02","AK","195","Petersburg","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",27.429000000000002,"A","CEC Survey",2017,15,"I",46.163007,"TON",8,{"v":1.6829999999999998,"d":"1.68"},{"$f":"VLOOKUP(A1314,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965353,"d":"1.64"}]
["02195","02","AK","195","Petersburg","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",18.732000000000003,"A","CEC Survey",2017,15,"I",31.525956000000004,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1315,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02195","02","AK","195","Petersburg","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,200.7,"A","CEC Survey",2017,15,"I",202.66685999999999,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1316,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02195","02","AK","195","Petersburg","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",100.35,"A","CEC Survey",2017,15,"I",25.0875,"TON",8,0.25,{"$f":"VLOOKUP(A1317,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02195","02","AK","195","Petersburg","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1318,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02195","02","AK","195","Petersburg","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",145.17299999999997,"A","CEC Survey",2017,15,"I",488.6523179999999,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1319,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02195","02","AK","195","Petersburg","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",192.00299999999996,"A","CEC Survey",2017,15,"I",646.2820979999999,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1320,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02195","02","AK","195","Petersburg","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",131.124,"A","CEC Survey",2017,15,"I",441.363384,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1321,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",48.321999999999996,"A","CEC Survey",2017,15,"I",162.651852,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1322,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.251859723698194,"d":"3.25"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.9179999999999997,"A","CEC Survey",2017,15,"I",13.187987999999999,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1323,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.251859723698194,"d":"3.25"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008610","Hydronic heater: outdoor","Hydronic heater",47.016,"A","CEC Survey",2017,15,"I",158.255856,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1324,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.251859723698194,"d":"3.25"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008620","Hydronic heater: indoor","Hydronic heater",30.038,"A","CEC Survey",2017,15,"I",101.10790800000001,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1325,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.251859723698194,"d":"3.25"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.306,"A","CEC Survey",2017,15,"I",4.395996,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1326,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.251859723698194,"d":"3.25"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008100","Fireplace: general","Fireplace: general",522.4,"A","CEC Survey",2017,15,"I",439.5996,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1327,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":0.8129649309245485,"d":"0.81"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",40.486,"A","CEC Survey",2017,15,"I",68.137938,"TON",8,{"v":1.6830000000000003,"d":"1.68"},{"$f":"VLOOKUP(A1328,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":1.6259298618490972,"d":"1.63"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",53.54599999999999,"A","CEC Survey",2017,15,"I",90.117918,"TON",8,{"v":1.6830000000000003,"d":"1.68"},{"$f":"VLOOKUP(A1329,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":1.6259298618490972,"d":"1.63"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",36.568000000000005,"A","CEC Survey",2017,15,"I",61.54394400000001,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1330,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":1.625929861849097,"d":"1.63"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,391.8,"A","CEC Survey",2017,15,"I",395.63964,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1331,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":0.9755579171094582,"d":"0.98"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",195.9,"A","CEC Survey",2017,15,"I",48.975,"TON",8,0.25,{"$f":"VLOOKUP(A1332,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":0.24152255820693655,"d":"0.24"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1333,cordwood_density!A:D,4,FALSE)","v":1.0351},{"$error":"#DIV/0!"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",283.402,"A","CEC Survey",2017,15,"I",953.931132,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1334,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981943,"d":"3.25"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",374.82199999999995,"A","CEC Survey",2017,15,"I",1261.650852,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1335,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981943,"d":"3.25"}]
["02198","02","AK","198","Prince of Wales-Hyder","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",255.976,"A","CEC Survey",2017,15,"I",861.6152160000001,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1336,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981943,"d":"3.25"}]
["02220","02","AK","220","Sitka","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1337,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02220","02","AK","220","Sitka","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1338,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02220","02","AK","220","Sitka","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1339,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02220","02","AK","220","Sitka","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1340,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02220","02","AK","220","Sitka","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1341,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02220","02","AK","220","Sitka","","2104008100","Fireplace: general","Fireplace: general",703,"A","CEC Survey",2017,15,"I",591.5745000000001,"TON",8,{"v":0.8415000000000001,"d":"0.84"},{"$f":"VLOOKUP(A1342,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482679,"d":"0.82"}]
["02220","02","AK","220","Sitka","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",217.93,"A","CEC Survey",2017,15,"I",366.77619000000004,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1343,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02220","02","AK","220","Sitka","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",288.22999999999996,"A","CEC Survey",2017,15,"I",485.09109,"TON",8,{"v":1.6830000000000003,"d":"1.68"},{"$f":"VLOOKUP(A1344,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965357,"d":"1.64"}]
["02220","02","AK","220","Sitka","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",196.84000000000003,"A","CEC Survey",2017,15,"I",331.28172000000006,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1345,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02220","02","AK","220","Sitka","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,527.25,"A","CEC Survey",2017,15,"I",532.4170499999999,"TON",8,{"v":1.0097999999999998,"d":"1.01"},{"$f":"VLOOKUP(A1346,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579211,"d":"0.98"}]
["02220","02","AK","220","Sitka","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$f":"P1347/J1347","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A1347,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S1347/T1347","v":{"$error":"#DIV/0!"}}]
["02220","02","AK","220","Sitka","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1348,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02220","02","AK","220","Sitka","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",381.3775,"A","CEC Survey",2017,15,"I",1283.716665,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1349,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02220","02","AK","220","Sitka","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",504.4025,"A","CEC Survey",2017,15,"I",1697.8188149999999,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1350,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02220","02","AK","220","Sitka","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",344.47,"A","CEC Survey",2017,15,"I",1159.48602,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1351,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",1.9018,"A","CEC Survey",2017,15,"I",6.4014588,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1352,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.15419999999999998,"A","CEC Survey",2017,15,"I",0.5190372,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1353,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008610","Hydronic heater: outdoor","Hydronic heater",1.8503999999999998,"A","CEC Survey",2017,15,"I",6.2284464,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1354,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008620","Hydronic heater: indoor","Hydronic heater",1.1822,"A","CEC Survey",2017,15,"I",3.9792852,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1355,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.0514,"A","CEC Survey",2017,15,"I",0.1730124,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1356,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008100","Fireplace: general","Fireplace: general",128.5,"A","CEC Survey",2017,15,"I",108.13275,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1357,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02230","02","AK","230","Skagway","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",7.9670000000000005,"A","CEC Survey",2017,15,"I",13.408461,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1358,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02230","02","AK","230","Skagway","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",10.537,"A","CEC Survey",2017,15,"I",17.733771,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1359,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02230","02","AK","230","Skagway","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",7.1960000000000015,"A","CEC Survey",2017,15,"I",12.110868000000002,"TON",8,{"v":1.6829999999999998,"d":"1.68"},{"$f":"VLOOKUP(A1360,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965353,"d":"1.64"}]
["02230","02","AK","230","Skagway","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,77.1,"A","CEC Survey",2017,15,"I",77.85558,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1361,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02230","02","AK","230","Skagway","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",15.42,"A","CEC Survey",2017,15,"I",3.855,"TON",8,0.25,{"$f":"VLOOKUP(A1362,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02230","02","AK","230","Skagway","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1363,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02230","02","AK","230","Skagway","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",39.835,"A","CEC Survey",2017,15,"I",134.08461,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1364,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",52.684999999999995,"A","CEC Survey",2017,15,"I",177.33771,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1365,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02230","02","AK","230","Skagway","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",35.980000000000004,"A","CEC Survey",2017,15,"I",121.10868,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1366,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930705,"d":"3.28"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",19.794999999999998,"A","CEC Survey",2017,15,"I",133.25994,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1367,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.605,"A","CEC Survey",2017,15,"I",10.804860000000001,"TON",8,{"v":6.732000000000001,"d":"6.73"},{"$f":"VLOOKUP(A1368,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386143,"d":"6.55"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008610","Hydronic heater: outdoor","Hydronic heater",19.259999999999998,"A","CEC Survey",2017,15,"I",129.65832,"TON",8,{"v":6.732000000000001,"d":"6.73"},{"$f":"VLOOKUP(A1369,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386143,"d":"6.55"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008620","Hydronic heater: indoor","Hydronic heater",12.305,"A","CEC Survey",2017,15,"I",82.83726000000001,"TON",8,{"v":6.732000000000001,"d":"6.73"},{"$f":"VLOOKUP(A1370,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386143,"d":"6.55"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.535,"A","CEC Survey",2017,15,"I",3.6016200000000005,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1371,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008100","Fireplace: general","Fireplace: general",107,"A","CEC Survey",2017,15,"I",540.243,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1372,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",82.925,"A","CEC Survey",2017,15,"I",488.4697125,"TON",8,{"v":5.8905,"d":"5.89"},{"$f":"VLOOKUP(A1373,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.732288828337874,"d":"5.73"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",109.675,"A","CEC Survey",2017,15,"I",646.0405875,"TON",8,{"v":5.8905,"d":"5.89"},{"$f":"VLOOKUP(A1374,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.732288828337874,"d":"5.73"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",74.9,"A","CEC Survey",2017,15,"I",441.19845000000004,"TON",8,{"v":5.8905,"d":"5.89"},{"$f":"VLOOKUP(A1375,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.732288828337874,"d":"5.73"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,428,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A1376,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0,"d":"0.00"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",53.5,"A","CEC Survey",2017,15,"I",13.375,"TON",8,0.25,{"$f":"VLOOKUP(A1377,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02240","02","AK","240","Southeast Fairbanks","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1378,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",290.23749999999995,"A","CEC Survey",2017,15,"I",1465.4091374999998,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1379,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",383.86249999999995,"A","CEC Survey",2017,15,"I",1938.1217624999997,"TON",8,{"v":5.0489999999999995,"d":"5.05"},{"$f":"VLOOKUP(A1380,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289606,"d":"4.91"}]
["02240","02","AK","240","Southeast Fairbanks","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",262.15,"A","CEC Survey",2017,15,"I",1323.59535,"TON",8,{"v":5.049,"d":"5.05"},{"$f":"VLOOKUP(A1381,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":4.913390424289607,"d":"4.91"}]
["02261","02","AK","261","Valdez Cordova","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1382,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02261","02","AK","261","Valdez Cordova","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1383,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02261","02","AK","261","Valdez Cordova","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1384,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02261","02","AK","261","Valdez Cordova","","2104008620","Hydronic heater: indoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1385,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02261","02","AK","261","Valdez Cordova","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1386,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02261","02","AK","261","Valdez Cordova","","2104008100","Fireplace: general","Fireplace: general",757.2,"A","CEC Survey",2017,15,"I",637.1838,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1387,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02261","02","AK","261","Valdez Cordova","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",234.732,"A","CEC Survey",2017,15,"I",395.053956,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1388,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02261","02","AK","261","Valdez Cordova","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",310.452,"A","CEC Survey",2017,15,"I",522.490716,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1389,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02261","02","AK","261","Valdez Cordova","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",212.01600000000002,"A","CEC Survey",2017,15,"I",356.82292800000005,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1390,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02261","02","AK","261","Valdez Cordova","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1391,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02261","02","AK","261","Valdez Cordova","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",56.79,"A","CEC Survey",2017,15,"I",14.1975,"TON",8,0.25,{"$f":"VLOOKUP(A1392,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02261","02","AK","261","Valdez Cordova","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1393,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02261","02","AK","261","Valdez Cordova","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",352.09799999999996,"A","CEC Survey",2017,15,"I",1185.1618680000001,"TON",8,{"v":3.366000000000001,"d":"3.37"},{"$f":"VLOOKUP(A1394,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193072,"d":"3.28"}]
["02261","02","AK","261","Valdez Cordova","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",465.67799999999994,"A","CEC Survey",2017,15,"I",1567.472148,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1395,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02261","02","AK","261","Valdez Cordova","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",318.024,"A","CEC Survey",2017,15,"I",1070.4687840000001,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1396,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02275","02","AK","275","Wrangell","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",20.072499999999998,"A","CEC Survey",2017,15,"I",67.564035,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1397,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981943,"d":"3.25"}]
["02275","02","AK","275","Wrangell","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.6275,"A","CEC Survey",2017,15,"I",5.478165,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1398,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.251859723698194,"d":"3.25"}]
["02275","02","AK","275","Wrangell","","2104008610","Hydronic heater: outdoor","Hydronic heater",19.529999999999998,"A","CEC Survey",2017,15,"I",65.73798,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1399,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.251859723698194,"d":"3.25"}]
["02275","02","AK","275","Wrangell","","2104008620","Hydronic heater: indoor","Hydronic heater",12.477500000000001,"A","CEC Survey",2017,15,"I",41.999265,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1400,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981934,"d":"3.25"}]
["02275","02","AK","275","Wrangell","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.5425,"A","CEC Survey",2017,15,"I",1.8260550000000002,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1401,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981943,"d":"3.25"}]
["02275","02","AK","275","Wrangell","","2104008100","Fireplace: general","Fireplace: general",217,"A","CEC Survey",2017,15,"I",182.6055,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1402,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":0.8129649309245485,"d":"0.81"}]
["02275","02","AK","275","Wrangell","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",67.27,"A","CEC Survey",2017,15,"I",113.21541,"TON",8,{"v":1.6830000000000003,"d":"1.68"},{"$f":"VLOOKUP(A1403,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":1.6259298618490972,"d":"1.63"}]
["02275","02","AK","275","Wrangell","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",88.97,"A","CEC Survey",2017,15,"I",149.73651,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1404,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":1.625929861849097,"d":"1.63"}]
["02275","02","AK","275","Wrangell","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",60.760000000000005,"A","CEC Survey",2017,15,"I",102.25908000000001,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1405,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":1.625929861849097,"d":"1.63"}]
["02275","02","AK","275","Wrangell","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,162.75,"A","CEC Survey",2017,15,"I",164.34494999999998,"TON",8,{"v":1.0097999999999998,"d":"1.01"},{"$f":"VLOOKUP(A1406,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":0.9755579171094579,"d":"0.98"}]
["02275","02","AK","275","Wrangell","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",81.375,"A","CEC Survey",2017,15,"I",20.34375,"TON",8,0.25,{"$f":"VLOOKUP(A1407,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":0.24152255820693655,"d":"0.24"}]
["02275","02","AK","275","Wrangell","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1408,cordwood_density!A:D,4,FALSE)","v":1.0351},{"$error":"#DIV/0!"}]
["02275","02","AK","275","Wrangell","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",117.7225,"A","CEC Survey",2017,15,"I",396.25393499999996,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1409,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981934,"d":"3.25"}]
["02275","02","AK","275","Wrangell","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",155.6975,"A","CEC Survey",2017,15,"I",524.077785,"TON",8,{"v":3.3659999999999997,"d":"3.37"},{"$f":"VLOOKUP(A1410,cordwood_density!A:D,4,FALSE)","v":1.0351},{"v":3.2518597236981934,"d":"3.25"}]
["02275","02","AK","275","Wrangell","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",106.33000000000001,"A","CEC Survey",2017,15,"I",357.90678,"TON",8,{"$f":"P1411/J1411","v":{"v":3.3659999999999997,"d":"3.37"}},{"$f":"VLOOKUP(A1411,cordwood_density!A:D,4,FALSE)","v":1.0351},{"$f":"S1411/T1411","v":{"v":3.2518597236981934,"d":"3.25"}}]
["02282","02","AK","282","Yakutat","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",4.4585,"A","CEC Survey",2017,15,"I",15.007311000000001,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1412,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02282","02","AK","282","Yakutat","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.3615,"A","CEC Survey",2017,15,"I",1.216809,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1413,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02282","02","AK","282","Yakutat","","2104008610","Hydronic heater: outdoor","Hydronic heater",4.338,"A","CEC Survey",2017,15,"I",14.601708000000002,"TON",8,{"v":3.3660000000000005,"d":"3.37"},{"$f":"VLOOKUP(A1414,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.2755936161930714,"d":"3.28"}]
["02282","02","AK","282","Yakutat","","2104008620","Hydronic heater: indoor","Hydronic heater",2.7715,"A","CEC Survey",2017,15,"I",9.328869000000001,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1415,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02282","02","AK","282","Yakutat","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.12050000000000001,"A","CEC Survey",2017,15,"I",0.40560300000000005,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1416,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02282","02","AK","282","Yakutat","","2104008100","Fireplace: general","Fireplace: general",48.2,"A","CEC Survey",2017,15,"I",40.560300000000005,"TON",8,{"v":0.8415,"d":"0.84"},{"$f":"VLOOKUP(A1417,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8188984040482677,"d":"0.82"}]
["02282","02","AK","282","Yakutat","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",14.942,"A","CEC Survey",2017,15,"I",25.147386000000004,"TON",8,{"v":1.6830000000000003,"d":"1.68"},{"$f":"VLOOKUP(A1418,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965357,"d":"1.64"}]
["02282","02","AK","282","Yakutat","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",19.762,"A","CEC Survey",2017,15,"I",33.259446000000004,"TON",8,{"v":1.6830000000000003,"d":"1.68"},{"$f":"VLOOKUP(A1419,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965357,"d":"1.64"}]
["02282","02","AK","282","Yakutat","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",13.496000000000002,"A","CEC Survey",2017,15,"I",22.713768000000005,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1420,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02282","02","AK","282","Yakutat","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,36.15,"A","CEC Survey",2017,15,"I",36.50427,"TON",8,{"v":1.0098,"d":"1.01"},{"$f":"VLOOKUP(A1421,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579213,"d":"0.98"}]
["02282","02","AK","282","Yakutat","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",18.075,"A","CEC Survey",2017,15,"I",4.51875,"TON",8,0.25,{"$f":"VLOOKUP(A1422,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24328532502919423,"d":"0.24"}]
["02282","02","AK","282","Yakutat","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1423,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02282","02","AK","282","Yakutat","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",26.1485,"A","CEC Survey",2017,15,"I",88.015851,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1424,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02282","02","AK","282","Yakutat","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",34.583499999999994,"A","CEC Survey",2017,15,"I",116.40806099999999,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1425,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02282","02","AK","282","Yakutat","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",23.618000000000002,"A","CEC Survey",2017,15,"I",79.49818800000001,"TON",8,{"v":3.366,"d":"3.37"},{"$f":"VLOOKUP(A1426,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.275593616193071,"d":"3.28"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",15.8138,"A","CEC Survey",2017,15,"I",106.4585016,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1427,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.2822,"A","CEC Survey",2017,15,"I",8.6317704,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1428,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008610","Hydronic heater: outdoor","Hydronic heater",15.3864,"A","CEC Survey",2017,15,"I",103.5812448,"TON",8,{"v":6.731999999999999,"d":"6.73"},{"$f":"VLOOKUP(A1429,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386141,"d":"6.55"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008620","Hydronic heater: indoor","Hydronic heater",9.830200000000001,"A","CEC Survey",2017,15,"I",66.17690640000001,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1430,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.4274,"A","CEC Survey",2017,15,"I",2.8772568,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1431,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008100","Fireplace: general","Fireplace: general",128.22,"A","CEC Survey",2017,15,"I",215.79426,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1432,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",33.1235,"A","CEC Survey",2017,15,"I",55.7468505,"TON",8,{"v":1.683,"d":"1.68"},{"$f":"VLOOKUP(A1433,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965355,"d":"1.64"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",43.8085,"A","CEC Survey",2017,15,"I",73.7297055,"TON",8,{"v":1.6829999999999998,"d":"1.68"},{"$f":"VLOOKUP(A1434,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965353,"d":"1.64"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",29.918000000000006,"A","CEC Survey",2017,15,"I",50.351994000000005,"TON",8,{"v":1.6829999999999998,"d":"1.68"},{"$f":"VLOOKUP(A1435,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6377968080965353,"d":"1.64"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,534.25,"A","CEC Survey",2017,15,"I",539.4856500000001,"TON",8,{"v":1.0098000000000003,"d":"1.01"},{"$f":"VLOOKUP(A1436,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9826780848579215,"d":"0.98"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1437,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02290","02","AK","290","Yukon Koyukuk","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A1438,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",298.1115,"A","CEC Survey",2017,15,"I",2006.886618,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1439,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",394.27649999999994,"A","CEC Survey",2017,15,"I",2654.269398,"TON",8,{"v":6.732000000000001,"d":"6.73"},{"$f":"VLOOKUP(A1440,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386143,"d":"6.55"}]
["02290","02","AK","290","Yukon Koyukuk","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",269.262,"A","CEC Survey",2017,15,"I",1812.6717840000001,"TON",8,{"v":6.732,"d":"6.73"},{"$f":"VLOOKUP(A1441,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":6.551187232386142,"d":"6.55"}]
["04001","04","AZ","001","Apache","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",147.73214616926143,"A","CEC Survey",2017,15,"I",171.7933981180692,"TON",8,{"v":1.162870794019604,"d":"1.16"},{"$f":"VLOOKUP(A1442,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":1.1565099890796657,"d":"1.16"}]
["04001","04","AZ","001","Apache","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.978282121832006,"A","CEC Survey",2017,15,"I",13.929194442005612,"TON",8,{"v":1.162870794019604,"d":"1.16"},{"$f":"VLOOKUP(A1443,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":1.1565099890796657,"d":"1.16"}]
["04001","04","AZ","001","Apache","","2104008610","Hydronic heater: outdoor","Hydronic heater",143.73938546198409,"A","CEC Survey",2017,15,"I",167.15033330406735,"TON",8,{"v":1.162870794019604,"d":"1.16"},{"$f":"VLOOKUP(A1444,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":1.1565099890796657,"d":"1.16"}]
["04001","04","AZ","001","Apache","","2104008620","Hydronic heater: indoor","Hydronic heater",91.83349626737872,"A","CEC Survey",2017,15,"I",106.79049072204303,"TON",8,{"v":1.162870794019604,"d":"1.16"},{"$f":"VLOOKUP(A1445,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":1.1565099890796657,"d":"1.16"}]
["04001","04","AZ","001","Apache","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.9927607072773355,"A","CEC Survey",2017,15,"I",4.643064814001871,"TON",8,{"v":1.1628707940196041,"d":"1.16"},{"$f":"VLOOKUP(A1446,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":1.156509989079666,"d":"1.16"}]
["04001","04","AZ","001","Apache","","2104008100","Fireplace: general","Fireplace: general",799.65495162,"A","CEC Survey",2017,15,"I",156.41504891430782,"TON",8,{"v":0.195603176842,"d":"0.20"},{"$f":"VLOOKUP(A1447,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.19453324399999997,"d":"0.19"}]
["04001","04","AZ","001","Apache","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",430.7776302249,"A","CEC Survey",2017,15,"I",78.67592753285797,"TON",8,{"v":0.182636984868,"d":"0.18"},{"$f":"VLOOKUP(A1448,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.181637976,"d":"0.18"}]
["04001","04","AZ","001","Apache","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",569.7381561039,"A","CEC Survey",2017,15,"I",104.05525899507022,"TON",8,{"v":0.18263698486800004,"d":"0.18"},{"$f":"VLOOKUP(A1449,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.18163797600000003,"d":"0.18"}]
["04001","04","AZ","001","Apache","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",389.08947246120005,"A","CEC Survey",2017,15,"I",71.0621280941943,"TON",8,{"v":0.18263698486800004,"d":"0.18"},{"$f":"VLOOKUP(A1450,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.18163797600000003,"d":"0.18"}]
["04001","04","AZ","001","Apache","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2752.6767275700004,"A","CEC Survey",2017,15,"I",344.927328594157,"TON",8,{"v":0.125306152059,"d":"0.13"},{"$f":"VLOOKUP(A1451,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.124620738,"d":"0.12"}]
["04001","04","AZ","001","Apache","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",745.7638696199999,"A","CEC Survey",2017,15,"I",162.45288189368796,"TON",8,{"v":0.21783420800000003,"d":"0.22"},{"$f":"VLOOKUP(A1452,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.21664267329686723,"d":"0.22"}]
["04001","04","AZ","001","Apache","","2104009000","Wax Log; Total: All Combustor Types",null,369.82718463079243,"A","CEC Survey",2017,15,"I",288.64804657209953,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A1453,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.7762251616111386,"d":"0.78"}]
["04001","04","AZ","001","Apache","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",921.5325587663999,"A","CEC Survey",2017,15,"I",567.6487301515701,"TON",8,{"v":0.615983368956,"d":"0.62"},{"$f":"VLOOKUP(A1454,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.612613992,"d":"0.61"}]
["04001","04","AZ","001","Apache","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1218.8011261103998,"A","CEC Survey",2017,15,"I",750.7612237488509,"TON",8,{"v":0.6159833689560001,"d":"0.62"},{"$f":"VLOOKUP(A1455,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.6126139920000001,"d":"0.61"}]
["04001","04","AZ","001","Apache","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",832.3519885632,"A","CEC Survey",2017,15,"I",512.714982072386,"TON",8,{"v":0.615983368956,"d":"0.62"},{"$f":"VLOOKUP(A1456,cordwood_density!A:D,4,FALSE)","v":1.0055},{"v":0.612613992,"d":"0.61"}]
["04003","04","AZ","003","Cochise","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",81.68695564298712,"A","CEC Survey",2017,15,"I",79.15467059909841,"TON",8,{"v":0.9690001295316224,"d":"0.97"},{"$f":"VLOOKUP(A1457,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9528024872483997,"d":"0.95"}]
["04003","04","AZ","003","Cochise","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.623266673755712,"A","CEC Survey",2017,15,"I",6.417946264791763,"TON",8,{"v":0.9690001295316225,"d":"0.97"},{"$f":"VLOOKUP(A1458,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9528024872483998,"d":"0.95"}]
["04003","04","AZ","003","Cochise","","2104008610","Hydronic heater: outdoor","Hydronic heater",79.47920008506854,"A","CEC Survey",2017,15,"I",77.01535517750115,"TON",8,{"v":0.9690001295316224,"d":"0.97"},{"$f":"VLOOKUP(A1459,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9528024872483997,"d":"0.95"}]
["04003","04","AZ","003","Cochise","","2104008620","Hydronic heater: indoor","Hydronic heater",50.77837783212713,"A","CEC Survey",2017,15,"I",49.204254696736854,"TON",8,{"v":0.9690001295316225,"d":"0.97"},{"$f":"VLOOKUP(A1460,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9528024872483998,"d":"0.95"}]
["04003","04","AZ","003","Cochise","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.2077555579185706,"A","CEC Survey",2017,15,"I",2.1393154215972543,"TON",8,{"v":0.9690001295316224,"d":"0.97"},{"$f":"VLOOKUP(A1461,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9528024872483997,"d":"0.95"}]
["04003","04","AZ","003","Cochise","","2104008100","Fireplace: general","Fireplace: general",2831.2357474,"A","CEC Survey",2017,15,"I",545.7895400049755,"TON",8,{"v":0.192774317895,"d":"0.19"},{"$f":"VLOOKUP(A1462,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.189551935,"d":"0.19"}]
["04003","04","AZ","003","Cochise","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",672.306840888,"A","CEC Survey",2017,15,"I",109.60234161013241,"TON",8,{"v":0.16302428436599997,"d":"0.16"},{"$f":"VLOOKUP(A1463,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.16029919799999998,"d":"0.16"}]
["04003","04","AZ","003","Cochise","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",889.1800153679999,"A","CEC Survey",2017,15,"I",144.95793567791705,"TON",8,{"v":0.16302428436599997,"d":"0.16"},{"$f":"VLOOKUP(A1464,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.16029919799999998,"d":"0.16"}]
["04003","04","AZ","003","Cochise","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",607.244888544,"A","CEC Survey",2017,15,"I",98.99566338979703,"TON",8,{"v":0.163024284366,"d":"0.16"},{"$f":"VLOOKUP(A1465,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.160299198,"d":"0.16"}]
["04003","04","AZ","003","Cochise","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5932.751159240001,"A","CEC Survey",2017,15,"I",752.9931714159525,"TON",8,{"v":0.12692141490599998,"d":"0.13"},{"$f":"VLOOKUP(A1466,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.12479981799999999,"d":"0.12"}]
["04003","04","AZ","003","Cochise","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1368.4548758,"A","CEC Survey",2017,15,"I",80.45720829030549,"TON",8,{"v":0.058794199,"d":"0.06"},{"$f":"VLOOKUP(A1467,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.05781140511307768,"d":"0.06"}]
["04003","04","AZ","003","Cochise","","2104009000","Wax Log; Total: All Combustor Types",null,930.9116434434079,"A","CEC Survey",2017,15,"I",130.32763008207712,"TON",8,0.14,{"$f":"VLOOKUP(A1468,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.13765978367748283,"d":"0.14"}]
["04003","04","AZ","003","Cochise","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",911.9565458643999,"A","CEC Survey",2017,15,"I",453.67096850852136,"TON",8,{"v":0.497469940389,"d":"0.50"},{"$f":"VLOOKUP(A1469,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.48915431700000006,"d":"0.49"}]
["04003","04","AZ","003","Cochise","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1206.1360767883998,"A","CEC Survey",2017,15,"I",600.0164422209476,"TON",8,{"v":0.49746994038900005,"d":"0.50"},{"$f":"VLOOKUP(A1470,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.4891543170000001,"d":"0.49"}]
["04003","04","AZ","003","Cochise","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",823.7026865872,"A","CEC Survey",2017,15,"I",409.76732639479354,"TON",8,{"v":0.497469940389,"d":"0.50"},{"$f":"VLOOKUP(A1471,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.48915431700000006,"d":"0.49"}]
["04005","04","AZ","005","Coconino","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",170.59557147195324,"A","CEC Survey",2017,15,"I",190.4062322150377,"TON",8,{"v":1.1161264654888268,"d":"1.12"},{"$f":"VLOOKUP(A1472,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":1.0958531816286958,"d":"1.10"}]
["04005","04","AZ","005","Coconino","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.832073362590803,"A","CEC Survey",2017,15,"I",15.438343152570624,"TON",8,{"v":1.1161264654888268,"d":"1.12"},{"$f":"VLOOKUP(A1473,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":1.0958531816286958,"d":"1.10"}]
["04005","04","AZ","005","Coconino","","2104008610","Hydronic heater: outdoor","Hydronic heater",165.98488035108963,"A","CEC Survey",2017,15,"I",185.2601178308475,"TON",8,{"v":1.1161264654888268,"d":"1.12"},{"$f":"VLOOKUP(A1474,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":1.0958531816286958,"d":"1.10"}]
["04005","04","AZ","005","Coconino","","2104008620","Hydronic heater: indoor","Hydronic heater",106.04589577986283,"A","CEC Survey",2017,15,"I",118.3606308363748,"TON",8,{"$f":"P1475/J1475","v":{"v":1.1161264654888268,"d":"1.12"}},{"$f":"VLOOKUP(A1475,cordwood_density!A:D,4,FALSE)","v":1.0185},{"$f":"S1475/T1475","v":{"v":1.0958531816286958,"d":"1.10"}}]
["04005","04","AZ","005","Coconino","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.610691120863601,"A","CEC Survey",2017,15,"I",5.146114384190208,"TON",8,{"v":1.1161264654888268,"d":"1.12"},{"$f":"VLOOKUP(A1476,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":1.0958531816286958,"d":"1.10"}]
["04005","04","AZ","005","Coconino","","2104008100","Fireplace: general","Fireplace: general",3107.801058376,"A","CEC Survey",2017,15,"I",550.977411347405,"TON",8,{"v":0.1772885075325,"d":"0.18"},{"$f":"VLOOKUP(A1477,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.174068245,"d":"0.17"}]
["04005","04","AZ","005","Coconino","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",613.11292956312,"A","CEC Survey",2017,15,"I",113.07333426482636,"TON",8,{"v":0.18442497101699998,"d":"0.18"},{"$f":"VLOOKUP(A1478,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.181075082,"d":"0.18"}]
["04005","04","AZ","005","Coconino","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",810.8912939383199,"A","CEC Survey",2017,15,"I",149.54860338251228,"TON",8,{"v":0.184424971017,"d":"0.18"},{"$f":"VLOOKUP(A1479,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.18107508200000003,"d":"0.18"}]
["04005","04","AZ","005","Coconino","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",553.7794202505601,"A","CEC Survey",2017,15,"I",102.13075352952059,"TON",8,{"v":0.18442497101699998,"d":"0.18"},{"$f":"VLOOKUP(A1480,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.181075082,"d":"0.18"}]
["04005","04","AZ","005","Coconino","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5591.8767177,"A","CEC Survey",2017,15,"I",704.0234262775696,"TON",8,{"v":0.125901099366,"d":"0.13"},{"$f":"VLOOKUP(A1481,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.123614236,"d":"0.12"}]
["04005","04","AZ","005","Coconino","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1277.524225056,"A","CEC Survey",2017,15,"I",169.64999329088053,"TON",8,{"v":0.132795911,"d":"0.13"},{"$f":"VLOOKUP(A1482,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.13038381050564554,"d":"0.13"}]
["04005","04","AZ","005","Coconino","","2104009000","Wax Log; Total: All Combustor Types",null,901.1436795806528,"A","CEC Survey",2017,15,"I",703.3375955080938,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A1483,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.7663175257731958,"d":"0.77"}]
["04005","04","AZ","005","Coconino","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1143.91673730548,"A","CEC Survey",2017,15,"I",624.2234431367438,"TON",8,{"v":0.5456895793019999,"d":"0.55"},{"$f":"VLOOKUP(A1484,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.5357776919999999,"d":"0.54"}]
["04005","04","AZ","005","Coconino","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1512.9221364362797,"A","CEC Survey",2017,15,"I",825.5858441485966,"TON",8,{"v":0.545689579302,"d":"0.55"},{"$f":"VLOOKUP(A1485,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.535777692,"d":"0.54"}]
["04005","04","AZ","005","Coconino","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1033.21511756624,"A","CEC Survey",2017,15,"I",563.814722833188,"TON",8,{"v":0.545689579302,"d":"0.55"},{"$f":"VLOOKUP(A1486,cordwood_density!A:D,4,FALSE)","v":1.0185},{"v":0.535777692,"d":"0.54"}]
["04007","04","AZ","007","Gila","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",58.78959898343224,"A","CEC Survey",2017,15,"I",61.06126581406424,"TON",8,{"v":1.0386406247008453,"d":"1.04"},{"$f":"VLOOKUP(A1487,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.0107440878754819,"d":"1.01"}]
["04007","04","AZ","007","Gila","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.766724241899912,"A","CEC Survey",2017,15,"I",4.950913444383587,"TON",8,{"v":1.038640624700845,"d":"1.04"},{"$f":"VLOOKUP(A1488,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.0107440878754816,"d":"1.01"}]
["04007","04","AZ","007","Gila","","2104008610","Hydronic heater: outdoor","Hydronic heater",57.20069090279893,"A","CEC Survey",2017,15,"I",59.410961332603044,"TON",8,{"v":1.0386406247008453,"d":"1.04"},{"$f":"VLOOKUP(A1489,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.0107440878754819,"d":"1.01"}]
["04007","04","AZ","007","Gila","","2104008620","Hydronic heater: indoor","Hydronic heater",36.54488585456599,"A","CEC Survey",2017,15,"I",37.9570030736075,"TON",8,{"v":1.0386406247008453,"d":"1.04"},{"$f":"VLOOKUP(A1490,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.0107440878754819,"d":"1.01"}]
["04007","04","AZ","007","Gila","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.5889080806333038,"A","CEC Survey",2017,15,"I",1.6503044814611958,"TON",8,{"v":1.0386406247008453,"d":"1.04"},{"$f":"VLOOKUP(A1491,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.0107440878754819,"d":"1.01"}]
["04007","04","AZ","007","Gila","","2104008100","Fireplace: general","Fireplace: general",1368.90895776,"A","CEC Survey",2017,15,"I",262.1708007017354,"TON",8,{"v":0.1915180693468,"d":"0.19"},{"$f":"VLOOKUP(A1492,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.186374143,"d":"0.19"}]
["04007","04","AZ","007","Gila","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",384.0323145552,"A","CEC Survey",2017,15,"I",73.55820397734296,"TON",8,{"v":0.1915417041468,"d":"0.19"},{"$f":"VLOOKUP(A1493,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.186397143,"d":"0.19"}]
["04007","04","AZ","007","Gila","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",507.9137063472,"A","CEC Survey",2017,15,"I",97.28665687326003,"TON",8,{"v":0.1915417041468,"d":"0.19"},{"$f":"VLOOKUP(A1494,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.186397143,"d":"0.19"}]
["04007","04","AZ","007","Gila","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",346.86789701760006,"A","CEC Survey",2017,15,"I",66.43966810856783,"TON",8,{"v":0.19154170414679997,"d":"0.19"},{"$f":"VLOOKUP(A1495,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.18639714299999996,"d":"0.19"}]
["04007","04","AZ","007","Gila","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2920.844577345,"A","CEC Survey",2017,15,"I",375.93416557131593,"TON",8,{"v":0.1287073500888,"d":"0.13"},{"$f":"VLOOKUP(A1496,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.125250438,"d":"0.13"}]
["04007","04","AZ","007","Gila","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",688.40069175,"A","CEC Survey",2017,15,"I",63.34153542451397,"TON",8,{"v":0.092012597,"d":"0.09"},{"$f":"VLOOKUP(A1497,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.08954125827170105,"d":"0.09"}]
["04007","04","AZ","007","Gila","","2104009000","Wax Log; Total: All Combustor Types",null,408.7414121994703,"A","CEC Survey",2017,15,"I",57.22379770792585,"TON",8,0.14,{"$f":"VLOOKUP(A1498,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.1362397820163488,"d":"0.14"}]
["04007","04","AZ","007","Gila","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",558.0715176882,"A","CEC Survey",2017,15,"I",301.6040206343163,"TON",8,{"v":0.5404397305272001,"d":"0.54"},{"$f":"VLOOKUP(A1499,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.525924222,"d":"0.53"}]
["04007","04","AZ","007","Gila","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",738.0945879102,"A","CEC Survey",2017,15,"I",398.8956401937732,"TON",8,{"v":0.5404397305272001,"d":"0.54"},{"$f":"VLOOKUP(A1500,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.525924222,"d":"0.53"}]
["04007","04","AZ","007","Gila","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",504.06459662160006,"A","CEC Survey",2017,15,"I",272.4165347664793,"TON",8,{"v":0.5404397305272,"d":"0.54"},{"$f":"VLOOKUP(A1501,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5259242219999999,"d":"0.53"}]
["04009","04","AZ","009","Graham","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",19.29462871722106,"A","CEC Survey",2017,15,"I",18.947435355533834,"TON",8,{"v":0.9820056987477896,"d":"0.98"},{"$f":"VLOOKUP(A1502,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9556303024015079,"d":"0.96"}]
["04009","04","AZ","009","Graham","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.5644293554503559,"A","CEC Survey",2017,15,"I",1.5362785423405811,"TON",8,{"v":0.9820056987477898,"d":"0.98"},{"$f":"VLOOKUP(A1503,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.955630302401508,"d":"0.96"}]
["04009","04","AZ","009","Graham","","2104008610","Hydronic heater: outdoor","Hydronic heater",18.77315226540427,"A","CEC Survey",2017,15,"I",18.435342508086972,"TON",8,{"v":0.9820056987477896,"d":"0.98"},{"$f":"VLOOKUP(A1504,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9556303024015079,"d":"0.96"}]
["04009","04","AZ","009","Graham","","2104008620","Hydronic heater: indoor","Hydronic heater",11.993958391786064,"A","CEC Survey",2017,15,"I",11.778135491277789,"TON",8,{"v":0.9820056987477896,"d":"0.98"},{"$f":"VLOOKUP(A1505,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9556303024015079,"d":"0.96"}]
["04009","04","AZ","009","Graham","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.5214764518167854,"A","CEC Survey",2017,15,"I",0.5120928474468603,"TON",8,{"v":0.9820056987477895,"d":"0.98"},{"$f":"VLOOKUP(A1506,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9556303024015078,"d":"0.96"}]
["04009","04","AZ","009","Graham","","2104008100","Fireplace: general","Fireplace: general",660.0960582719999,"A","CEC Survey",2017,15,"I",128.95196612971765,"TON",8,{"v":0.1953533345848,"d":"0.20"},{"$f":"VLOOKUP(A1507,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.19010639799999998,"d":"0.19"}]
["04009","04","AZ","009","Graham","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",159.00635495584,"A","CEC Survey",2017,15,"I",27.049762588795733,"TON",8,{"v":0.1701174937084,"d":"0.17"},{"$f":"VLOOKUP(A1508,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.165548359,"d":"0.17"}]
["04009","04","AZ","009","Graham","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",210.29872752224,"A","CEC Survey",2017,15,"I",35.775492456149195,"TON",8,{"v":0.1701174937084,"d":"0.17"},{"$f":"VLOOKUP(A1509,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.165548359,"d":"0.17"}]
["04009","04","AZ","009","Graham","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",143.61864318592,"A","CEC Survey",2017,15,"I",24.432043628589696,"TON",8,{"v":0.17011749370840004,"d":"0.17"},{"$f":"VLOOKUP(A1510,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.16554835900000003,"d":"0.17"}]
["04009","04","AZ","009","Graham","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1339.315030592,"A","CEC Survey",2017,15,"I",171.64981001151418,"TON",8,{"v":0.1281623860636,"d":"0.13"},{"$f":"VLOOKUP(A1511,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.124720111,"d":"0.12"}]
["04009","04","AZ","009","Graham","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",307.192369568,"A","CEC Survey",2017,15,"I",19.19834225053138,"TON",8,{"v":0.062496156,"d":"0.06"},{"$f":"VLOOKUP(A1512,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.0608175905021409,"d":"0.06"}]
["04009","04","AZ","009","Graham","","2104009000","Wax Log; Total: All Combustor Types",null,207.8455288534346,"A","CEC Survey",2017,15,"I",29.098374039480845,"TON",8,0.14,{"$f":"VLOOKUP(A1513,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.1362397820163488,"d":"0.14"}]
["04009","04","AZ","009","Graham","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",212.49098123456,"A","CEC Survey",2017,15,"I",110.00391681145736,"TON",8,{"v":0.51768746218,"d":"0.52"},{"$f":"VLOOKUP(A1514,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5037830499999999,"d":"0.50"}]
["04009","04","AZ","009","Graham","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",281.03645905215996,"A","CEC Survey",2017,15,"I",145.48905126676618,"TON",8,{"v":0.5176874621800001,"d":"0.52"},{"$f":"VLOOKUP(A1515,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.50378305,"d":"0.50"}]
["04009","04","AZ","009","Graham","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",191.92733788928,"A","CEC Survey",2017,15,"I",99.35837647486473,"TON",8,{"v":0.51768746218,"d":"0.52"},{"$f":"VLOOKUP(A1516,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5037830499999999,"d":"0.50"}]
["04011","04","AZ","011","Greenlee","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",6.759207687288303,"A","CEC Survey",2017,15,"I",6.39167966141701,"TON",8,{"v":0.9456255758256276,"d":"0.95"},{"$f":"VLOOKUP(A1517,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.9253601877146761,"d":"0.93"}]
["04011","04","AZ","011","Greenlee","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.5480438665368894,"A","CEC Survey",2017,15,"I",0.5182442968716494,"TON",8,{"v":0.9456255758256276,"d":"0.95"},{"$f":"VLOOKUP(A1518,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.9253601877146761,"d":"0.93"}]
["04011","04","AZ","011","Greenlee","","2104008610","Hydronic heater: outdoor","Hydronic heater",6.576526398442673,"A","CEC Survey",2017,15,"I",6.218931562459794,"TON",8,{"v":0.9456255758256277,"d":"0.95"},{"$f":"VLOOKUP(A1519,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.9253601877146762,"d":"0.93"}]
["04011","04","AZ","011","Greenlee","","2104008620","Hydronic heater: indoor","Hydronic heater",4.201669643449486,"A","CEC Survey",2017,15,"I",3.9732062760159796,"TON",8,{"v":0.9456255758256277,"d":"0.95"},{"$f":"VLOOKUP(A1520,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.9253601877146762,"d":"0.93"}]
["04011","04","AZ","011","Greenlee","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.1826812888456298,"A","CEC Survey",2017,15,"I",0.1727480989572165,"TON",8,{"v":0.9456255758256276,"d":"0.95"},{"$f":"VLOOKUP(A1521,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.9253601877146761,"d":"0.93"}]
["04011","04","AZ","011","Greenlee","","2104008100","Fireplace: general","Fireplace: general",298.879612544,"A","CEC Survey",2017,15,"I",57.79258420324257,"TON",8,{"v":0.19336408967920002,"d":"0.19"},{"$f":"VLOOKUP(A1522,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.18922016800000002,"d":"0.19"}]
["04011","04","AZ","011","Greenlee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",46.35538929536,"A","CEC Survey",2017,15,"I",8.969162590397211,"TON",8,{"v":0.19348694351909995,"d":"0.19"},{"$f":"VLOOKUP(A1523,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.18934038899999994,"d":"0.19"}]
["04011","04","AZ","011","Greenlee","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",61.30874068095999,"A","CEC Survey",2017,15,"I",11.862440845364054,"TON",8,{"v":0.19348694351909998,"d":"0.19"},{"$f":"VLOOKUP(A1524,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.18934038899999997,"d":"0.19"}]
["04011","04","AZ","011","Greenlee","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",41.86938387968,"A","CEC Survey",2017,15,"I",8.10117911390716,"TON",8,{"v":0.19348694351909998,"d":"0.19"},{"$f":"VLOOKUP(A1525,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.18934038899999997,"d":"0.19"}]
["04011","04","AZ","011","Greenlee","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,432.88264852,"A","CEC Survey",2017,15,"I",55.304529439517296,"TON",8,{"v":0.12775871157830002,"d":"0.13"},{"$f":"VLOOKUP(A1526,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.125020757,"d":"0.13"}]
["04011","04","AZ","011","Greenlee","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",100.547544648,"A","CEC Survey",2017,15,"I",6.629247725175907,"TON",8,{"v":0.065931473,"d":"0.07"},{"$f":"VLOOKUP(A1527,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.06451851746746257,"d":"0.06"}]
["04011","04","AZ","011","Greenlee","","2104009000","Wax Log; Total: All Combustor Types",null,63.70192775719333,"A","CEC Survey",2017,15,"I",49.71899788369395,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A1528,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.7637678833545356,"d":"0.76"}]
["04011","04","AZ","011","Greenlee","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",62.62979808072,"A","CEC Survey",2017,15,"I",34.00491372614332,"TON",8,{"v":0.5429510355807999,"d":"0.54"},{"$f":"VLOOKUP(A1529,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.531315232,"d":"0.53"}]
["04011","04","AZ","011","Greenlee","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",82.83295875192,"A","CEC Survey",2017,15,"I",44.974240734576654,"TON",8,{"v":0.5429510355807999,"d":"0.54"},{"$f":"VLOOKUP(A1530,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.531315232,"d":"0.53"}]
["04011","04","AZ","011","Greenlee","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",56.56884987936001,"A","CEC Survey",2017,15,"I",30.714115623613328,"TON",8,{"v":0.5429510355807999,"d":"0.54"},{"$f":"VLOOKUP(A1531,cordwood_density!A:D,4,FALSE)","v":1.0219},{"v":0.531315232,"d":"0.53"}]
["04012","04","AZ","012","La Paz","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",11.762066773537152,"A","CEC Survey",2017,15,"I",12.247062187259685,"TON",8,{"v":1.0412338599210895,"d":"1.04"},{"$f":"VLOOKUP(A1532,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.013267672169219,"d":"1.01"}]
["04012","04","AZ","012","La Paz","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.9536810897462555,"A","CEC Survey",2017,15,"I",0.9930050422102447,"TON",8,{"v":1.0412338599210895,"d":"1.04"},{"$f":"VLOOKUP(A1533,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.013267672169219,"d":"1.01"}]
["04012","04","AZ","012","La Paz","","2104008610","Hydronic heater: outdoor","Hydronic heater",11.444173076955066,"A","CEC Survey",2017,15,"I",11.916060506522935,"TON",8,{"v":1.0412338599210895,"d":"1.04"},{"$f":"VLOOKUP(A1534,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.013267672169219,"d":"1.01"}]
["04012","04","AZ","012","La Paz","","2104008620","Hydronic heater: indoor","Hydronic heater",7.311555021387959,"A","CEC Survey",2017,15,"I",7.61303865694521,"TON",8,{"v":1.0412338599210895,"d":"1.04"},{"$f":"VLOOKUP(A1535,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.013267672169219,"d":"1.01"}]
["04012","04","AZ","012","La Paz","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.31789369658208516,"A","CEC Survey",2017,15,"I",0.33100168073674824,"TON",8,{"v":1.0412338599210897,"d":"1.04"},{"$f":"VLOOKUP(A1536,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.0132676721692193,"d":"1.01"}]
["04012","04","AZ","012","La Paz","","2104008100","Fireplace: general","Fireplace: general",201.44106673200002,"A","CEC Survey",2017,15,"I",42.45781543653376,"TON",8,{"v":0.2107704060812,"d":"0.21"},{"$f":"VLOOKUP(A1537,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.205109387,"d":"0.21"}]
["04012","04","AZ","012","La Paz","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",161.26661381308,"A","CEC Survey",2017,15,"I",21.669407244571012,"TON",8,{"v":0.13437007655960004,"d":"0.13"},{"$f":"VLOOKUP(A1538,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.13076107100000003,"d":"0.13"}]
["04012","04","AZ","012","La Paz","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",213.28810213987998,"A","CEC Survey",2017,15,"I",28.659538613787465,"TON",8,{"$f":"P1539/J1539","v":{"v":0.13437007655960004,"d":"0.13"}},{"$f":"VLOOKUP(A1539,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S1539/T1539","v":{"v":0.13076107100000003,"d":"0.13"}}]
["04012","04","AZ","012","La Paz","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",145.66016731504,"A","CEC Survey",2017,15,"I",19.572367833806076,"TON",8,{"v":0.13437007655960004,"d":"0.13"},{"$f":"VLOOKUP(A1540,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.13076107100000003,"d":"0.13"}]
["04012","04","AZ","012","La Paz","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,847.236657642,"A","CEC Survey",2017,15,"I",108.13941554206107,"TON",8,{"v":0.1276377911256,"d":"0.13"},{"$f":"VLOOKUP(A1541,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.124209606,"d":"0.12"}]
["04012","04","AZ","012","La Paz","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",191.19522386199998,"A","CEC Survey",2017,15,"I",11.745296015910702,"TON",8,{"v":0.061430907,"d":"0.06"},{"$f":"VLOOKUP(A1542,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.05978095270533281,"d":"0.06"}]
["04012","04","AZ","012","La Paz","","2104009000","Wax Log; Total: All Combustor Types",null,166.60212853977018,"A","CEC Survey",2017,15,"I",39.00693953991203,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1543,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22784381082133123,"d":"0.23"}]
["04012","04","AZ","012","La Paz","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",197.49209226222,"A","CEC Survey",2017,15,"I",106.92858894833724,"TON",8,{"v":0.5414322554564001,"d":"0.54"},{"$f":"VLOOKUP(A1544,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.526890089,"d":"0.53"}]
["04012","04","AZ","012","La Paz","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",261.19921879842,"A","CEC Survey",2017,15,"I",141.42168215747827,"TON",8,{"v":0.5414322554564001,"d":"0.54"},{"$f":"VLOOKUP(A1545,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.526890089,"d":"0.53"}]
["04012","04","AZ","012","La Paz","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",178.37995430136004,"A","CEC Survey",2017,15,"I",96.58066098559493,"TON",8,{"v":0.5414322554564001,"d":"0.54"},{"$f":"VLOOKUP(A1546,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.526890089,"d":"0.53"}]
["04013","04","AZ","013","Maricopa","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",1272.3075826805255,"A","CEC Survey",2017,15,"I",1168.5791685708145,"TON",8,{"v":0.918472218886589,"d":"0.92"},{"$f":"VLOOKUP(A1547,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.902586693088236,"d":"0.90"}]
["04013","04","AZ","013","Maricopa","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",103.16007427139395,"A","CEC Survey",2017,15,"I",94.74966231655253,"TON",8,{"v":0.918472218886589,"d":"0.92"},{"$f":"VLOOKUP(A1548,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.902586693088236,"d":"0.90"}]
["04013","04","AZ","013","Maricopa","","2104008610","Hydronic heater: outdoor","Hydronic heater",1237.9208912567274,"A","CEC Survey",2017,15,"I",1136.9959477986304,"TON",8,{"v":0.9184722188865891,"d":"0.92"},{"$f":"VLOOKUP(A1549,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.9025866930882361,"d":"0.90"}]
["04013","04","AZ","013","Maricopa","","2104008620","Hydronic heater: indoor","Hydronic heater",790.8939027473536,"A","CEC Survey",2017,15,"I",726.4140777602361,"TON",8,{"v":0.918472218886589,"d":"0.92"},{"$f":"VLOOKUP(A1550,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.902586693088236,"d":"0.90"}]
["04013","04","AZ","013","Maricopa","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",34.386691423797984,"A","CEC Survey",2017,15,"I",31.583220772184177,"TON",8,{"v":0.918472218886589,"d":"0.92"},{"$f":"VLOOKUP(A1551,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.902586693088236,"d":"0.90"}]
["04013","04","AZ","013","Maricopa","","2104008100","Fireplace: general","Fireplace: general",68608.806042795,"A","CEC Survey",2017,15,"I",10828.8570522263,"TON",8,{"v":0.1578347981376,"d":"0.16"},{"$f":"VLOOKUP(A1552,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.155104951,"d":"0.16"}]
["04013","04","AZ","013","Maricopa","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",20473.338481137478,"A","CEC Survey",2017,15,"I",3470.7904393578206,"TON",8,{"v":0.16952733148800003,"d":"0.17"},{"$f":"VLOOKUP(A1553,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.16659525500000003,"d":"0.17"}]
["04013","04","AZ","013","Maricopa","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",27077.64121698828,"A","CEC Survey",2017,15,"I",4590.400258505504,"TON",8,{"v":0.169527331488,"d":"0.17"},{"$f":"VLOOKUP(A1554,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.166595255,"d":"0.17"}]
["04013","04","AZ","013","Maricopa","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",18492.047660382243,"A","CEC Survey",2017,15,"I",3134.9074936135153,"TON",8,{"v":0.169527331488,"d":"0.17"},{"$f":"VLOOKUP(A1555,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.166595255,"d":"0.17"}]
["04013","04","AZ","013","Maricopa","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,159492.323913804,"A","CEC Survey",2017,15,"I",20685.953808555052,"TON",8,{"v":0.12969874224,"d":"0.13"},{"$f":"VLOOKUP(A1556,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.127455525,"d":"0.13"}]
["04013","04","AZ","013","Maricopa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",31937.516465235,"A","CEC Survey",2017,15,"I",1602.2395694645038,"TON",8,{"v":0.050167945,"d":"0.05"},{"$f":"VLOOKUP(A1557,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.049300260416666665,"d":"0.05"}]
["04013","04","AZ","013","Maricopa","","2104009000","Wax Log; Total: All Combustor Types",null,22306.963827395524,"A","CEC Survey",2017,15,"I",5222.7807469249165,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A1558,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.23008284198113202,"d":"0.23"}]
["04013","04","AZ","013","Maricopa","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",21087.58976111067,"A","CEC Survey",2017,15,"I",7887.341571320582,"TON",8,{"v":0.374027646624,"d":"0.37"},{"$f":"VLOOKUP(A1559,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.367558615,"d":"0.37"}]
["04013","04","AZ","013","Maricopa","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",27890.03807114637,"A","CEC Survey",2017,15,"I",10431.645304004642,"TON",8,{"v":0.374027646624,"d":"0.37"},{"$f":"VLOOKUP(A1560,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.367558615,"d":"0.37"}]
["04013","04","AZ","013","Maricopa","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",19046.85526809996,"A","CEC Survey",2017,15,"I",7124.050451515365,"TON",8,{"v":0.374027646624,"d":"0.37"},{"$f":"VLOOKUP(A1561,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.367558615,"d":"0.37"}]
["04015","04","AZ","015","Mohave","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",142.0785821206459,"A","CEC Survey",2017,15,"I",144.8293653999757,"TON",8,{"v":1.0193609989505241,"d":"1.02"},{"$f":"VLOOKUP(A1562,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":1.0022229858917748,"d":"1.00"}]
["04015","04","AZ","015","Mohave","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.519885036809129,"A","CEC Survey",2017,15,"I",11.74292151891695,"TON",8,{"v":1.0193609989505241,"d":"1.02"},{"$f":"VLOOKUP(A1563,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":1.0022229858917748,"d":"1.00"}]
["04015","04","AZ","015","Mohave","","2104008610","Hydronic heater: outdoor","Hydronic heater",138.23862044170954,"A","CEC Survey",2017,15,"I",140.91505822700339,"TON",8,{"v":1.0193609989505241,"d":"1.02"},{"$f":"VLOOKUP(A1564,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":1.0022229858917748,"d":"1.00"}]
["04015","04","AZ","015","Mohave","","2104008620","Hydronic heater: indoor","Hydronic heater",88.31911861553665,"A","CEC Survey",2017,15,"I",90.02906497836328,"TON",8,{"v":1.0193609989505241,"d":"1.02"},{"$f":"VLOOKUP(A1565,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":1.0022229858917748,"d":"1.00"}]
["04015","04","AZ","015","Mohave","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.839961678936376,"A","CEC Survey",2017,15,"I",3.9143071729723165,"TON",8,{"v":1.0193609989505241,"d":"1.02"},{"$f":"VLOOKUP(A1566,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":1.0022229858917748,"d":"1.00"}]
["04015","04","AZ","015","Mohave","","2104008100","Fireplace: general","Fireplace: general",3779.9028988585146,"A","CEC Survey",2017,15,"I",697.7049049389052,"TON",8,{"v":0.18458275876599997,"d":"0.18"},{"$f":"VLOOKUP(A1567,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.18147945999999998,"d":"0.18"}]
["04015","04","AZ","015","Mohave","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1321.0835062652754,"A","CEC Survey",2017,15,"I",207.0152698058201,"TON",8,{"v":0.15670112360350003,"d":"0.16"},{"$f":"VLOOKUP(A1568,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.15406658500000003,"d":"0.15"}]
["04015","04","AZ","015","Mohave","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1747.2394760282675,"A","CEC Survey",2017,15,"I",273.79438909802013,"TON",8,{"v":0.1567011236035,"d":"0.16"},{"$f":"VLOOKUP(A1569,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.154066585,"d":"0.15"}]
["04015","04","AZ","015","Mohave","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1193.236715336378,"A","CEC Survey",2017,15,"I",186.98153401816012,"TON",8,{"v":0.1567011236035,"d":"0.16"},{"$f":"VLOOKUP(A1570,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.154066585,"d":"0.15"}]
["04015","04","AZ","015","Mohave","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,9704.373807556633,"A","CEC Survey",2017,15,"I",1229.0052274983177,"TON",8,{"v":0.1266444648434,"d":"0.13"},{"$f":"VLOOKUP(A1571,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.12451525400000002,"d":"0.12"}]
["04015","04","AZ","015","Mohave","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2108.2123503132707,"A","CEC Survey",2017,15,"I",143.2276189203284,"TON",8,{"v":0.067937947,"d":"0.07"},{"$f":"VLOOKUP(A1572,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.06679573984858914,"d":"0.07"}]
["04015","04","AZ","015","Mohave","","2104009000","Wax Log; Total: All Combustor Types",null,1588.798794090682,"A","CEC Survey",2017,15,"I",371.9891158976777,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1573,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.23019594926752532,"d":"0.23"}]
["04015","04","AZ","015","Mohave","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1726.6529675123338,"A","CEC Survey",2017,15,"I",842.0849208095195,"TON",8,{"v":0.48769783891359997,"d":"0.49"},{"$f":"VLOOKUP(A1574,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.47949841600000004,"d":"0.48"}]
["04015","04","AZ","015","Mohave","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2283.6377957421187,"A","CEC Survey",2017,15,"I",1113.7252178448484,"TON",8,{"v":0.4876978389136,"d":"0.49"},{"$f":"VLOOKUP(A1575,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.4794984160000001,"d":"0.48"}]
["04015","04","AZ","015","Mohave","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1559.5575190433985,"A","CEC Survey",2017,15,"I",760.5928316989209,"TON",8,{"v":0.4876978389135999,"d":"0.49"},{"$f":"VLOOKUP(A1576,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.479498416,"d":"0.48"}]
["04017","04","AZ","017","Navajo","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",186.52574619726718,"A","CEC Survey",2017,15,"I",216.29349854314967,"TON",8,{"v":1.1595905817441443,"d":"1.16"},{"$f":"VLOOKUP(A1577,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.1284454863216662,"d":"1.13"}]
["04017","04","AZ","017","Navajo","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",15.123709151129772,"A","CEC Survey",2017,15,"I",17.53731069268781,"TON",8,{"v":1.1595905817441443,"d":"1.16"},{"$f":"VLOOKUP(A1578,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.1284454863216662,"d":"1.13"}]
["04017","04","AZ","017","Navajo","","2104008610","Hydronic heater: outdoor","Hydronic heater",181.48450981355725,"A","CEC Survey",2017,15,"I",210.44772831225373,"TON",8,{"v":1.1595905817441443,"d":"1.16"},{"$f":"VLOOKUP(A1579,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.1284454863216662,"d":"1.13"}]
["04017","04","AZ","017","Navajo","","2104008620","Hydronic heater: indoor","Hydronic heater",115.94843682532826,"A","CEC Survey",2017,15,"I",134.45271531060655,"TON",8,{"v":1.1595905817441443,"d":"1.16"},{"$f":"VLOOKUP(A1580,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.1284454863216662,"d":"1.13"}]
["04017","04","AZ","017","Navajo","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.041236383709924,"A","CEC Survey",2017,15,"I",5.845770230895937,"TON",8,{"v":1.1595905817441443,"d":"1.16"},{"$f":"VLOOKUP(A1581,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.1284454863216662,"d":"1.13"}]
["04017","04","AZ","017","Navajo","","2104008100","Fireplace: general","Fireplace: general",1676.997324996,"A","CEC Survey",2017,15,"I",320.13833061722977,"TON",8,{"v":0.19089972646080003,"d":"0.19"},{"$f":"VLOOKUP(A1582,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.18577240800000003,"d":"0.19"}]
["04017","04","AZ","017","Navajo","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",610.3423087106099,"A","CEC Survey",2017,15,"I",106.59895411357216,"TON",8,{"v":0.17465437442600001,"d":"0.17"},{"$f":"VLOOKUP(A1583,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.169963385,"d":"0.17"}]
["04017","04","AZ","017","Navajo","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",807.2269244237099,"A","CEC Survey",2017,15,"I",140.98571350504704,"TON",8,{"v":0.17465437442600001,"d":"0.17"},{"$f":"VLOOKUP(A1584,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.169963385,"d":"0.17"}]
["04017","04","AZ","017","Navajo","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",551.27692399668,"A","CEC Survey",2017,15,"I",96.2829262961297,"TON",8,{"v":0.17465437442600001,"d":"0.17"},{"$f":"VLOOKUP(A1585,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.169963385,"d":"0.17"}]
["04017","04","AZ","017","Navajo","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4574.741151435,"A","CEC Survey",2017,15,"I",585.664368957124,"TON",8,{"v":0.1280213130252,"d":"0.13"},{"$f":"VLOOKUP(A1586,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.124582827,"d":"0.12"}]
["04017","04","AZ","017","Navajo","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1157.796862551,"A","CEC Survey",2017,15,"I",192.91849038336656,"TON",8,{"v":0.166625508,"d":"0.17"},{"$f":"VLOOKUP(A1587,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.16215016348773842,"d":"0.16"}]
["04017","04","AZ","017","Navajo","","2104009000","Wax Log; Total: All Combustor Types",null,648.5893958417446,"A","CEC Survey",2017,15,"I",506.2203913538649,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A1588,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["04017","04","AZ","017","Navajo","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1229.79354105993,"A","CEC Survey",2017,15,"I",729.4433062574348,"TON",8,{"v":0.5931428991152001,"d":"0.59"},{"$f":"VLOOKUP(A1589,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5772118520000001,"d":"0.58"}]
["04017","04","AZ","017","Navajo","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1626.50113495023,"A","CEC Survey",2017,15,"I",964.7475985985426,"TON",8,{"v":0.5931428991152,"d":"0.59"},{"$f":"VLOOKUP(A1590,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.577211852,"d":"0.58"}]
["04017","04","AZ","017","Navajo","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1110.78126289284,"A","CEC Survey",2017,15,"I",658.8520185551024,"TON",8,{"v":0.5931428991152001,"d":"0.59"},{"$f":"VLOOKUP(A1591,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5772118520000001,"d":"0.58"}]
["04019","04","AZ","019","Pima","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",405.70700200670007,"A","CEC Survey",2017,15,"I",386.4963607434402,"TON",8,{"v":0.952648977788797,"d":"0.95"},{"$f":"VLOOKUP(A1592,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9367246585927208,"d":"0.94"}]
["04019","04","AZ","019","Pima","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",32.89516232486757,"A","CEC Survey",2017,15,"I",31.337542762981638,"TON",8,{"v":0.952648977788797,"d":"0.95"},{"$f":"VLOOKUP(A1593,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9367246585927208,"d":"0.94"}]
["04019","04","AZ","019","Pima","","2104008610","Hydronic heater: outdoor","Hydronic heater",394.7419478984109,"A","CEC Survey",2017,15,"I",376.05051315577964,"TON",8,{"v":0.9526489777887969,"d":"0.95"},{"$f":"VLOOKUP(A1594,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9367246585927207,"d":"0.94"}]
["04019","04","AZ","019","Pima","","2104008620","Hydronic heater: indoor","Hydronic heater",252.19624449065142,"A","CEC Survey",2017,15,"I",240.25449451619258,"TON",8,{"v":0.9526489777887969,"d":"0.95"},{"$f":"VLOOKUP(A1595,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9367246585927207,"d":"0.94"}]
["04019","04","AZ","019","Pima","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.965054108289191,"A","CEC Survey",2017,15,"I",10.445847587660547,"TON",8,{"v":0.952648977788797,"d":"0.95"},{"$f":"VLOOKUP(A1596,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9367246585927208,"d":"0.94"}]
["04019","04","AZ","019","Pima","","2104008100","Fireplace: general","Fireplace: general",23879.08028847,"A","CEC Survey",2017,15,"I",4195.0239363780365,"TON",8,{"v":0.175677785145,"d":"0.18"},{"$f":"VLOOKUP(A1597,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.172741185,"d":"0.17"}]
["04019","04","AZ","019","Pima","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",4462.9931144634,"A","CEC Survey",2017,15,"I",745.4733125391818,"TON",8,{"v":0.167034385539,"d":"0.17"},{"$f":"VLOOKUP(A1598,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.164242267,"d":"0.16"}]
["04019","04","AZ","019","Pima","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",5902.6683126774,"A","CEC Survey",2017,15,"I",985.9485746485954,"TON",8,{"v":0.167034385539,"d":"0.17"},{"$f":"VLOOKUP(A1599,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.164242267,"d":"0.16"}]
["04019","04","AZ","019","Pima","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",4031.0905549992003,"A","CEC Survey",2017,15,"I",673.3307339063579,"TON",8,{"v":0.167034385539,"d":"0.17"},{"$f":"VLOOKUP(A1600,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.164242267,"d":"0.16"}]
["04019","04","AZ","019","Pima","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,42883.48070391,"A","CEC Survey",2017,15,"I",5387.31132851742,"TON",8,{"v":0.125626727124,"d":"0.13"},{"$f":"VLOOKUP(A1601,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.123526772,"d":"0.12"}]
["04019","04","AZ","019","Pima","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",8529.392861549999,"A","CEC Survey",2017,15,"I",405.64999215995675,"TON",8,{"v":0.04755907,"d":"0.05"},{"$f":"VLOOKUP(A1602,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.046764080629301874,"d":"0.05"}]
["04019","04","AZ","019","Pima","","2104009000","Wax Log; Total: All Combustor Types",null,7546.7090573942505,"A","CEC Survey",2017,15,"I",1056.5392680351952,"TON",8,{"$f":"P1603/J1603","v":0.14},{"$f":"VLOOKUP(A1603,cordwood_density!A:D,4,FALSE)","v":1.017},{"$f":"S1603/T1603","v":{"v":0.13765978367748283,"d":"0.14"}}]
["04019","04","AZ","019","Pima","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",5317.2756340275,"A","CEC Survey",2017,15,"I",2245.050087578672,"TON",8,{"v":0.42221811357899997,"d":"0.42"},{"$f":"VLOOKUP(A1604,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.415160387,"d":"0.42"}]
["04019","04","AZ","019","Pima","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",7032.525838552499,"A","CEC Survey",2017,15,"I",2969.2597932492113,"TON",8,{"v":0.42221811357899997,"d":"0.42"},{"$f":"VLOOKUP(A1605,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.415160387,"d":"0.42"}]
["04019","04","AZ","019","Pima","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",4802.70057267,"A","CEC Survey",2017,15,"I",2027.7871758775104,"TON",8,{"v":0.422218113579,"d":"0.42"},{"$f":"VLOOKUP(A1606,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.4151603870000001,"d":"0.42"}]
["04021","04","AZ","021","Pinal","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",164.9963998208266,"A","CEC Survey",2017,15,"I",155.80207347529011,"TON",8,{"v":0.9442755941613221,"d":"0.94"},{"$f":"VLOOKUP(A1607,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.9279437835704816,"d":"0.93"}]
["04021","04","AZ","021","Pinal","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.378086471958914,"A","CEC Survey",2017,15,"I",12.632600552050551,"TON",8,{"v":0.9442755941613222,"d":"0.94"},{"$f":"VLOOKUP(A1608,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.9279437835704817,"d":"0.93"}]
["04021","04","AZ","021","Pinal","","2104008610","Hydronic heater: outdoor","Hydronic heater",160.53703766350696,"A","CEC Survey",2017,15,"I",151.5912066246066,"TON",8,{"v":0.9442755941613222,"d":"0.94"},{"$f":"VLOOKUP(A1609,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.9279437835704817,"d":"0.93"}]
["04021","04","AZ","021","Pinal","","2104008620","Hydronic heater: indoor","Hydronic heater",102.56532961835168,"A","CEC Survey",2017,15,"I",96.8499375657209,"TON",8,{"v":0.9442755941613222,"d":"0.94"},{"$f":"VLOOKUP(A1610,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.9279437835704817,"d":"0.93"}]
["04021","04","AZ","021","Pinal","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.459362157319639,"A","CEC Survey",2017,15,"I",4.210866850683517,"TON",8,{"v":0.944275594161322,"d":"0.94"},{"$f":"VLOOKUP(A1611,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.9279437835704815,"d":"0.93"}]
["04021","04","AZ","021","Pinal","","2104008100","Fireplace: general","Fireplace: general",6846.101374145,"A","CEC Survey",2017,15,"I",1288.2681917748846,"TON",8,{"v":0.18817544780160003,"d":"0.19"},{"$f":"VLOOKUP(A1612,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.18492084100000003,"d":"0.18"}]
["04021","04","AZ","021","Pinal","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",2277.6784682591,"A","CEC Survey",2017,15,"I",368.3794775080383,"TON",8,{"v":0.16173462700799998,"d":"0.16"},{"$f":"VLOOKUP(A1613,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.15893732999999996,"d":"0.16"}]
["04021","04","AZ","021","Pinal","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3012.4134580201,"A","CEC Survey",2017,15,"I",487.2115670267603,"TON",8,{"v":0.16173462700799998,"d":"0.16"},{"$f":"VLOOKUP(A1614,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.15893732999999996,"d":"0.16"}]
["04021","04","AZ","021","Pinal","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",2057.2579713308,"A","CEC Survey",2017,15,"I",332.7298506524217,"TON",8,{"v":0.161734627008,"d":"0.16"},{"$f":"VLOOKUP(A1615,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.15893733,"d":"0.16"}]
["04021","04","AZ","021","Pinal","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,17545.475512818,"A","CEC Survey",2017,15,"I",2238.09645382013,"TON",8,{"v":0.12755974907519999,"d":"0.13"},{"$f":"VLOOKUP(A1616,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.12535352699999996,"d":"0.13"}]
["04021","04","AZ","021","Pinal","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",3787.406929751,"A","CEC Survey",2017,15,"I",174.88182579776176,"TON",8,{"v":0.046174554,"d":"0.05"},{"$f":"VLOOKUP(A1617,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.0453759375,"d":"0.05"}]
["04021","04","AZ","021","Pinal","","2104009000","Wax Log; Total: All Combustor Types",null,2627.418366700602,"A","CEC Survey",2017,15,"I",615.1635052578553,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1618,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.23008284198113205,"d":"0.23"}]
["04021","04","AZ","021","Pinal","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",2506.8950553021,"A","CEC Survey",2017,15,"I",1109.6650840707966,"TON",8,{"v":0.442645208352,"d":"0.44"},{"$f":"VLOOKUP(A1619,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.43498939499999995,"d":"0.43"}]
["04021","04","AZ","021","Pinal","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3315.5708795931,"A","CEC Survey",2017,15,"I",1467.6215628033117,"TON",8,{"v":0.442645208352,"d":"0.44"},{"$f":"VLOOKUP(A1620,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.43498939499999995,"d":"0.43"}]
["04021","04","AZ","021","Pinal","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2264.2923080148003,"A","CEC Survey",2017,15,"I",1002.2781404510422,"TON",8,{"v":0.442645208352,"d":"0.44"},{"$f":"VLOOKUP(A1621,cordwood_density!A:D,4,FALSE)","v":1.0176},{"v":0.43498939499999995,"d":"0.43"}]
["04023","04","AZ","023","Santa Cruz","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",29.493580735240087,"A","CEC Survey",2017,15,"I",28.632195715380544,"TON",8,{"v":0.970794152544851,"d":"0.97"},{"$f":"VLOOKUP(A1622,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9545665216763531,"d":"0.95"}]
["04023","04","AZ","023","Santa Cruz","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.3913714109654123,"A","CEC Survey",2017,15,"I",2.321529382328152,"TON",8,{"v":0.9707941525448511,"d":"0.97"},{"$f":"VLOOKUP(A1623,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9545665216763533,"d":"0.95"}]
["04023","04","AZ","023","Santa Cruz","","2104008610","Hydronic heater: outdoor","Hydronic heater",28.69645693158495,"A","CEC Survey",2017,15,"I",27.858352587937826,"TON",8,{"v":0.9707941525448509,"d":"0.97"},{"$f":"VLOOKUP(A1624,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.954566521676353,"d":"0.95"}]
["04023","04","AZ","023","Santa Cruz","","2104008620","Hydronic heater: indoor","Hydronic heater",18.333847484068166,"A","CEC Survey",2017,15,"I",17.7983919311825,"TON",8,{"v":0.9707941525448508,"d":"0.97"},{"$f":"VLOOKUP(A1625,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9545665216763529,"d":"0.95"}]
["04023","04","AZ","023","Santa Cruz","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7971238036551376,"A","CEC Survey",2017,15,"I",0.7738431274427174,"TON",8,{"v":0.9707941525448509,"d":"0.97"},{"$f":"VLOOKUP(A1626,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.954566521676353,"d":"0.95"}]
["04023","04","AZ","023","Santa Cruz","","2104008100","Fireplace: general","Fireplace: general",848.735149808,"A","CEC Survey",2017,15,"I",164.7200556626638,"TON",8,{"v":0.19407709896299996,"d":"0.19"},{"$f":"VLOOKUP(A1627,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.19083293899999998,"d":"0.19"}]
["04023","04","AZ","023","Santa Cruz","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",241.68354223552,"A","CEC Survey",2017,15,"I",43.38825329114669,"TON",8,{"v":0.17952506360099996,"d":"0.18"},{"$f":"VLOOKUP(A1628,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17652415299999996,"d":"0.18"}]
["04023","04","AZ","023","Santa Cruz","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",319.64597521472,"A","CEC Survey",2017,15,"I",57.38446403022627,"TON",8,{"v":0.17952506360099996,"d":"0.18"},{"$f":"VLOOKUP(A1629,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17652415299999996,"d":"0.18"}]
["04023","04","AZ","023","Santa Cruz","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",218.29481234176004,"A","CEC Survey",2017,15,"I",39.18939006942282,"TON",8,{"v":0.17952506360099996,"d":"0.18"},{"$f":"VLOOKUP(A1630,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17652415299999996,"d":"0.18"}]
["04023","04","AZ","023","Santa Cruz","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2040.378306736,"A","CEC Survey",2017,15,"I",257.3676378905906,"TON",8,{"v":0.126137215359,"d":"0.13"},{"$f":"VLOOKUP(A1631,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.124028727,"d":"0.12"}]
["04023","04","AZ","023","Santa Cruz","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",472.03074273600004,"A","CEC Survey",2017,15,"I",30.912564526313858,"TON",8,{"v":0.065488456,"d":"0.07"},{"$f":"VLOOKUP(A1632,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.06439376204523108,"d":"0.06"}]
["04023","04","AZ","023","Santa Cruz","","2104009000","Wax Log; Total: All Combustor Types",null,294.80131133293276,"A","CEC Survey",2017,15,"I",41.27218358661059,"TON",8,0.14,{"$f":"VLOOKUP(A1633,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.13765978367748283,"d":"0.14"}]
["04023","04","AZ","023","Santa Cruz","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",330.262650032,"A","CEC Survey",2017,15,"I",157.87611480601723,"TON",8,{"v":0.47803199904899996,"d":"0.48"},{"$f":"VLOOKUP(A1634,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.470041297,"d":"0.47"}]
["04023","04","AZ","023","Santa Cruz","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",436.798988752,"A","CEC Survey",2017,15,"I",208.8038937757002,"TON",8,{"v":0.47803199904899996,"d":"0.48"},{"$f":"VLOOKUP(A1635,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.470041297,"d":"0.47"}]
["04023","04","AZ","023","Santa Cruz","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",298.301748416,"A","CEC Survey",2017,15,"I",142.59778111511235,"TON",8,{"v":0.478031999049,"d":"0.48"},{"$f":"VLOOKUP(A1636,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.4700412970000001,"d":"0.47"}]
["04025","04","AZ","025","Yavapai","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",199.5850711971977,"A","CEC Survey",2017,15,"I",199.81467128504318,"TON",8,{"v":1.0011503870829028,"d":"1.00"},{"$f":"VLOOKUP(A1637,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.9843185400480807,"d":"0.98"}]
["04025","04","AZ","025","Yavapai","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",16.182573340313326,"A","CEC Survey",2017,15,"I",16.20118956365215,"TON",8,{"v":1.0011503870829028,"d":"1.00"},{"$f":"VLOOKUP(A1638,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.9843185400480807,"d":"0.98"}]
["04025","04","AZ","025","Yavapai","","2104008610","Hydronic heater: outdoor","Hydronic heater",194.1908800837599,"A","CEC Survey",2017,15,"I",194.41427476382577,"TON",8,{"v":1.0011503870829026,"d":"1.00"},{"$f":"VLOOKUP(A1639,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.9843185400480805,"d":"0.98"}]
["04025","04","AZ","025","Yavapai","","2104008620","Hydronic heater: indoor","Hydronic heater",124.06639560906885,"A","CEC Survey",2017,15,"I",124.20911998799981,"TON",8,{"v":1.0011503870829026,"d":"1.00"},{"$f":"VLOOKUP(A1640,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.9843185400480805,"d":"0.98"}]
["04025","04","AZ","025","Yavapai","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.394191113437776,"A","CEC Survey",2017,15,"I",5.400396521217383,"TON",8,{"v":1.0011503870829026,"d":"1.00"},{"$f":"VLOOKUP(A1641,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.9843185400480805,"d":"0.98"}]
["04025","04","AZ","025","Yavapai","","2104008100","Fireplace: general","Fireplace: general",5823.594514338721,"A","CEC Survey",2017,15,"I",1099.8181218516868,"TON",8,{"v":0.18885554602809998,"d":"0.19"},{"$f":"VLOOKUP(A1642,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.185680411,"d":"0.19"}]
["04025","04","AZ","025","Yavapai","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1300.3326887851795,"A","CEC Survey",2017,15,"I",218.32964202648657,"TON",8,{"v":0.1679029097011,"d":"0.17"},{"$f":"VLOOKUP(A1643,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.165080041,"d":"0.17"}]
["04025","04","AZ","025","Yavapai","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1719.794846457818,"A","CEC Survey",2017,15,"I",288.75855880922416,"TON",8,{"v":0.1679029097011,"d":"0.17"},{"$f":"VLOOKUP(A1644,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.165080041,"d":"0.17"}]
["04025","04","AZ","025","Yavapai","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1174.4940414833882,"A","CEC Survey",2017,15,"I",197.2009669916653,"TON",8,{"v":0.16790290970109997,"d":"0.17"},{"$f":"VLOOKUP(A1645,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.16508004099999998,"d":"0.17"}]
["04025","04","AZ","025","Yavapai","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,11711.383496561637,"A","CEC Survey",2017,15,"I",1475.911561488625,"TON",8,{"v":0.1260236727729,"d":"0.13"},{"$f":"VLOOKUP(A1646,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.12390489900000001,"d":"0.12"}]
["04025","04","AZ","025","Yavapai","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2655.086935220571,"A","CEC Survey",2017,15,"I",195.7769346227168,"TON",8,{"v":0.073736544,"d":"0.07"},{"$f":"VLOOKUP(A1647,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.07249684790089471,"d":"0.07"}]
["04025","04","AZ","025","Yavapai","","2104009000","Wax Log; Total: All Combustor Types",null,1786.5133679428866,"A","CEC Survey",2017,15,"I",250.11187151200414,"TON",8,0.14,{"$f":"VLOOKUP(A1648,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.13764624913971096,"d":"0.14"}]
["04025","04","AZ","025","Yavapai","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1917.2047625154935,"A","CEC Survey",2017,15,"I",974.6638769483272,"TON",8,{"v":0.5083775588317999,"d":"0.51"},{"$f":"VLOOKUP(A1649,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.499830458,"d":"0.50"}]
["04025","04","AZ","025","Yavapai","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2535.6579117140395,"A","CEC Survey",2017,15,"I",1289.071579189723,"TON",8,{"v":0.5083775588317999,"d":"0.51"},{"$f":"VLOOKUP(A1650,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.499830458,"d":"0.50"}]
["04025","04","AZ","025","Yavapai","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1731.6688177559297,"A","CEC Survey",2017,15,"I",880.3415662759086,"TON",8,{"v":0.5083775588317999,"d":"0.51"},{"$f":"VLOOKUP(A1651,cordwood_density!A:D,4,FALSE)","v":1.0171},{"v":0.499830458,"d":"0.50"}]
["04027","04","AZ","027","Yuma","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",59.909549836327656,"A","CEC Survey",2017,15,"I",59.07696069114045,"TON",8,{"v":0.986102563823934,"d":"0.99"},{"$f":"VLOOKUP(A1652,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9596171310081101,"d":"0.96"}]
["04027","04","AZ","027","Yuma","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.85753106781035,"A","CEC Survey",2017,15,"I",4.790023839822198,"TON",8,{"v":0.986102563823934,"d":"0.99"},{"$f":"VLOOKUP(A1653,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9596171310081101,"d":"0.96"}]
["04027","04","AZ","027","Yuma","","2104008610","Hydronic heater: outdoor","Hydronic heater",58.290372813724204,"A","CEC Survey",2017,15,"I",57.48028607786638,"TON",8,{"v":0.986102563823934,"d":"0.99"},{"$f":"VLOOKUP(A1654,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9596171310081101,"d":"0.96"}]
["04027","04","AZ","027","Yuma","","2104008620","Hydronic heater: indoor","Hydronic heater",37.241071519879355,"A","CEC Survey",2017,15,"I",36.723516105303524,"TON",8,{"v":0.986102563823934,"d":"0.99"},{"$f":"VLOOKUP(A1655,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9596171310081101,"d":"0.96"}]
["04027","04","AZ","027","Yuma","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.61917702260345,"A","CEC Survey",2017,15,"I",1.5966746132740661,"TON",8,{"v":0.986102563823934,"d":"0.99"},{"$f":"VLOOKUP(A1656,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9596171310081101,"d":"0.96"}]
["04027","04","AZ","027","Yuma","","2104008100","Fireplace: general","Fireplace: general",2359.73216988,"A","CEC Survey",2017,15,"I",439.5606529336194,"TON",8,{"v":0.1862756538832,"d":"0.19"},{"$f":"VLOOKUP(A1657,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.181272532,"d":"0.18"}]
["04027","04","AZ","027","Yuma","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1189.9695474633002,"A","CEC Survey",2017,15,"I",178.44094723229094,"TON",8,{"v":0.14995421320879998,"d":"0.15"},{"$f":"VLOOKUP(A1658,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.14592663799999997,"d":"0.15"}]
["04027","04","AZ","027","Yuma","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1573.8306918063,"A","CEC Survey",2017,15,"I",236.0025431136751,"TON",8,{"v":0.1499542132088,"d":"0.15"},{"$f":"VLOOKUP(A1659,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.145926638,"d":"0.15"}]
["04027","04","AZ","027","Yuma","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1074.8112041604002,"A","CEC Survey",2017,15,"I",161.17246846787572,"TON",8,{"v":0.1499542132088,"d":"0.15"},{"$f":"VLOOKUP(A1660,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.145926638,"d":"0.15"}]
["04027","04","AZ","027","Yuma","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,7285.35626802,"A","CEC Survey",2017,15,"I",929.2378951107619,"TON",8,{"v":0.1275487238956,"d":"0.13"},{"$f":"VLOOKUP(A1661,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.124122931,"d":"0.12"}]
["04027","04","AZ","027","Yuma","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1424.45071044,"A","CEC Survey",2017,15,"I",61.95758047763484,"TON",8,{"v":0.04349577,"d":"0.04"},{"$f":"VLOOKUP(A1662,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.042327530167380306,"d":"0.04"}]
["04027","04","AZ","027","Yuma","","2104009000","Wax Log; Total: All Combustor Types",null,1357.1691921397282,"A","CEC Survey",2017,15,"I",317.7571444448165,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A1663,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22784381082133126,"d":"0.23"}]
["04027","04","AZ","027","Yuma","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1164.7003130214,"A","CEC Survey",2017,15,"I",507.8387347850838,"TON",8,{"v":0.43602524109199997,"d":"0.44"},{"$f":"VLOOKUP(A1664,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.42431416999999994,"d":"0.42"}]
["04027","04","AZ","027","Yuma","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1540.4100914153998,"A","CEC Survey",2017,15,"I",671.6576814899495,"TON",8,{"v":0.436025241092,"d":"0.44"},{"$f":"VLOOKUP(A1665,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.42431417,"d":"0.42"}]
["04027","04","AZ","027","Yuma","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1051.9873795032001,"A","CEC Survey",2017,15,"I",458.6930507736241,"TON",8,{"v":0.43602524109199997,"d":"0.44"},{"$f":"VLOOKUP(A1666,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.42431416999999994,"d":"0.42"}]
["05001","05","AR","001","Arkansas","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",24.981240318435173,"A","CEC Survey",2017,15,"I",87.07165047041835,"TON",8,{"$f":"P1667/J1667","v":{"v":3.485481479723122,"d":"3.49"}},{"$f":"VLOOKUP(A1667,cordwood_density!A:D,4,FALSE)","v":1.2767},{"$f":"S1667/T1667","v":{"v":2.730070869995396,"d":"2.73"}}]
["05001","05","AR","001","Arkansas","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.025505971765014,"A","CEC Survey",2017,15,"I",7.059863551655541,"TON",8,{"v":3.4854814797231217,"d":"3.49"},{"$f":"VLOOKUP(A1668,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":2.7300708699953957,"d":"2.73"}]
["05001","05","AR","001","Arkansas","","2104008610","Hydronic heater: outdoor","Hydronic heater",24.306071661180166,"A","CEC Survey",2017,15,"I",84.7183626198665,"TON",8,{"v":3.4854814797231226,"d":"3.49"},{"$f":"VLOOKUP(A1669,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":2.7300708699953966,"d":"2.73"}]
["05001","05","AR","001","Arkansas","","2104008620","Hydronic heater: indoor","Hydronic heater",15.528879116865108,"A","CEC Survey",2017,15,"I",54.12562056269248,"TON",8,{"v":3.4854814797231217,"d":"3.49"},{"$f":"VLOOKUP(A1670,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":2.7300708699953957,"d":"2.73"}]
["05001","05","AR","001","Arkansas","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.6751686572550046,"A","CEC Survey",2017,15,"I",2.353287850551847,"TON",8,{"v":3.485481479723122,"d":"3.49"},{"$f":"VLOOKUP(A1671,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":2.730070869995396,"d":"2.73"}]
["05001","05","AR","001","Arkansas","","2104008100","Fireplace: general","Fireplace: general",712.919112864,"A","CEC Survey",2017,15,"I",417.0459857948529,"TON",8,{"v":0.584983595291,"d":"0.58"},{"$f":"VLOOKUP(A1672,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":0.45819972999999997,"d":"0.46"}]
["05001","05","AR","001","Arkansas","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",144.94456952376,"A","CEC Survey",2017,15,"I",124.22360702158912,"TON",8,{"v":0.857042160529,"d":"0.86"},{"$f":"VLOOKUP(A1673,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":0.67129487,"d":"0.67"}]
["05001","05","AR","001","Arkansas","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",191.70088227336,"A","CEC Survey",2017,15,"I",164.29573831887592,"TON",8,{"v":0.857042160529,"d":"0.86"},{"$f":"VLOOKUP(A1674,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":0.67129487,"d":"0.67"}]
["05001","05","AR","001","Arkansas","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",130.91767569888003,"A","CEC Survey",2017,15,"I",112.20196763240308,"TON",8,{"v":0.8570421605289998,"d":"0.86"},{"$f":"VLOOKUP(A1675,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":0.6712948699999999,"d":"0.67"}]
["05001","05","AR","001","Arkansas","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1051.156844352,"A","CEC Survey",2017,15,"I",450.22828278546257,"TON",8,{"v":0.42831693976459995,"d":"0.43"},{"$f":"VLOOKUP(A1676,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":0.335487538,"d":"0.34"}]
["05001","05","AR","001","Arkansas","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",234.82424511600001,"A","CEC Survey",2017,15,"I",79.30285134203147,"TON",8,{"v":0.337711514,"d":"0.34"},{"$f":"VLOOKUP(A1677,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":0.2645190835748414,"d":"0.26"}]
["05001","05","AR","001","Arkansas","","2104009000","Wax Log; Total: All Combustor Types",null,110.47998198281908,"A","CEC Survey",2017,15,"I",37.94200211238208,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1678,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":0.26899721939374954,"d":"0.27"}]
["05001","05","AR","001","Arkansas","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",200.5272466662,"A","CEC Survey",2017,15,"I",372.61267441102325,"TON",8,{"v":1.8581648160325996,"d":"1.86"},{"$f":"VLOOKUP(A1679,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":1.4554435779999997,"d":"1.46"}]
["05001","05","AR","001","Arkansas","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",265.2134552682,"A","CEC Survey",2017,15,"I",492.8103113178049,"TON",8,{"v":1.8581648160325996,"d":"1.86"},{"$f":"VLOOKUP(A1680,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":1.4554435779999997,"d":"1.46"}]
["05001","05","AR","001","Arkansas","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",181.12138408560003,"A","CEC Survey",2017,15,"I",336.55338333898874,"TON",8,{"v":1.8581648160325994,"d":"1.86"},{"$f":"VLOOKUP(A1681,cordwood_density!A:D,4,FALSE)","v":1.2767},{"v":1.4554435779999997,"d":"1.46"}]
["05003","05","AR","003","Ashley","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",35.58031067979957,"A","CEC Survey",2017,15,"I",128.45683755858818,"TON",8,{"v":3.6103349044537296,"d":"3.61"},{"$f":"VLOOKUP(A1682,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":2.713109569740535,"d":"2.71"}]
["05003","05","AR","003","Ashley","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.8848900551188836,"A","CEC Survey",2017,15,"I",10.415419261507148,"TON",8,{"v":3.610334904453729,"d":"3.61"},{"$f":"VLOOKUP(A1683,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":2.7131095697405345,"d":"2.71"}]
["05003","05","AR","003","Ashley","","2104008610","Hydronic heater: outdoor","Hydronic heater",34.6186806614266,"A","CEC Survey",2017,15,"I",124.98503113808579,"TON",8,{"v":3.6103349044537296,"d":"3.61"},{"$f":"VLOOKUP(A1684,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":2.713109569740535,"d":"2.71"}]
["05003","05","AR","003","Ashley","","2104008620","Hydronic heater: indoor","Hydronic heater",22.117490422578108,"A","CEC Survey",2017,15,"I",79.85154767155481,"TON",8,{"v":3.6103349044537296,"d":"3.61"},{"$f":"VLOOKUP(A1685,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":2.713109569740535,"d":"2.71"}]
["05003","05","AR","003","Ashley","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9616300183729612,"A","CEC Survey",2017,15,"I",3.471806420502383,"TON",8,{"v":3.610334904453729,"d":"3.61"},{"$f":"VLOOKUP(A1686,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":2.7131095697405345,"d":"2.71"}]
["05003","05","AR","003","Ashley","","2104008100","Fireplace: general","Fireplace: general",1018.9064564079999,"A","CEC Survey",2017,15,"I",608.1873304395898,"TON",8,{"v":0.5969020282624,"d":"0.60"},{"$f":"VLOOKUP(A1687,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":0.448562432,"d":"0.45"}]
["05003","05","AR","003","Ashley","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",200.47903248152002,"A","CEC Survey",2017,15,"I",241.10878109978077,"TON",8,{"v":1.2026633314983,"d":"1.20"},{"$f":"VLOOKUP(A1688,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":0.9037824689999999,"d":"0.90"}]
["05003","05","AR","003","Ashley","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",265.14968812072,"A","CEC Survey",2017,15,"I",318.88580726100037,"TON",8,{"v":1.2026633314983002,"d":"1.20"},{"$f":"VLOOKUP(A1689,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":0.9037824690000001,"d":"0.90"}]
["05003","05","AR","003","Ashley","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",181.07783578976003,"A","CEC Survey",2017,15,"I",217.7756732514149,"TON",8,{"v":1.2026633314983,"d":"1.20"},{"$f":"VLOOKUP(A1690,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":0.9037824689999999,"d":"0.90"}]
["05003","05","AR","003","Ashley","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1223.448266226,"A","CEC Survey",2017,15,"I",544.9909179391123,"TON",8,{"v":0.44545481242150003,"d":"0.45"},{"$f":"VLOOKUP(A1691,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":0.334752245,"d":"0.33"}]
["05003","05","AR","003","Ashley","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",272.491536142,"A","CEC Survey",2017,15,"I",125.28966136606586,"TON",8,{"v":0.459792855,"d":"0.46"},{"$f":"VLOOKUP(A1692,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":0.3455270571879462,"d":"0.35"}]
["05003","05","AR","003","Ashley","","2104009000","Wax Log; Total: All Combustor Types",null,117.51783834937933,"A","CEC Survey",2017,15,"I",27.514721783768387,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A1693,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":0.17594671977154883,"d":"0.18"}]
["05003","05","AR","003","Ashley","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",257.86685899276,"A","CEC Survey",2017,15,"I",550.3401361861804,"TON",8,{"v":2.1342026592166,"d":"2.13"},{"$f":"VLOOKUP(A1694,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":1.6038195380000002,"d":"1.60"}]
["05003","05","AR","003","Ashley","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",341.04971673235997,"A","CEC Survey",2017,15,"I",727.8692123752709,"TON",8,{"v":2.1342026592166,"d":"2.13"},{"$f":"VLOOKUP(A1695,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":1.6038195380000002,"d":"1.60"}]
["05003","05","AR","003","Ashley","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",232.91200167088002,"A","CEC Survey",2017,15,"I",497.0814133294533,"TON",8,{"v":2.1342026592166,"d":"2.13"},{"$f":"VLOOKUP(A1696,cordwood_density!A:D,4,FALSE)","v":1.3307},{"v":1.6038195380000002,"d":"1.60"}]
["05005","05","AR","005","Baxter","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",134.25587866802326,"A","CEC Survey",2017,15,"I",557.0627989565074,"TON",8,{"v":4.149261875779502,"d":"4.15"},{"$f":"VLOOKUP(A1697,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":2.940236589979806,"d":"2.94"}]
["05005","05","AR","005","Baxter","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.885611783893776,"A","CEC Survey",2017,15,"I",45.16725396944655,"TON",8,{"v":4.149261875779503,"d":"4.15"},{"$f":"VLOOKUP(A1698,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":2.940236589979807,"d":"2.94"}]
["05005","05","AR","005","Baxter","","2104008610","Hydronic heater: outdoor","Hydronic heater",130.62734140672532,"A","CEC Survey",2017,15,"I",542.0070476333585,"TON",8,{"v":4.149261875779502,"d":"4.15"},{"$f":"VLOOKUP(A1699,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":2.940236589979806,"d":"2.94"}]
["05005","05","AR","005","Baxter","","2104008620","Hydronic heater: indoor","Hydronic heater",83.4563570098523,"A","CEC Survey",2017,15,"I",346.28228043242353,"TON",8,{"v":4.149261875779502,"d":"4.15"},{"$f":"VLOOKUP(A1700,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":2.940236589979806,"d":"2.94"}]
["05005","05","AR","005","Baxter","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.6285372612979256,"A","CEC Survey",2017,15,"I",15.05575132314885,"TON",8,{"v":4.149261875779502,"d":"4.15"},{"$f":"VLOOKUP(A1701,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":2.940236589979806,"d":"2.94"}]
["05005","05","AR","005","Baxter","","2104008100","Fireplace: general","Fireplace: general",2183.662262804,"A","CEC Survey",2017,15,"I",1390.911455539124,"TON",8,{"v":0.6369627204864,"d":"0.64"},{"$f":"VLOOKUP(A1702,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":0.451362472,"d":"0.45"}]
["05005","05","AR","005","Baxter","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",452.9889318001,"A","CEC Survey",2017,15,"I",587.7264198752373,"TON",8,{"v":1.29744101592,"d":"1.30"},{"$f":"VLOOKUP(A1703,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":0.919388475,"d":"0.92"}]
["05005","05","AR","005","Baxter","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",599.1143936711,"A","CEC Survey",2017,15,"I",777.3155875769266,"TON",8,{"v":1.2974410159199998,"d":"1.30"},{"$f":"VLOOKUP(A1704,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":0.9193884749999999,"d":"0.92"}]
["05005","05","AR","005","Baxter","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",409.1512932388,"A","CEC Survey",2017,15,"I",530.8496695647304,"TON",8,{"v":1.2974410159199998,"d":"1.30"},{"$f":"VLOOKUP(A1705,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":0.9193884749999999,"d":"0.92"}]
["05005","05","AR","005","Baxter","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2849.286135718,"A","CEC Survey",2017,15,"I",1348.4025279755872,"TON",8,{"v":0.4732422311232,"d":"0.47"},{"$f":"VLOOKUP(A1706,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":0.335347386,"d":"0.34"}]
["05005","05","AR","005","Baxter","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",686.0589178719999,"A","CEC Survey",2017,15,"I",498.1208579151531,"TON",8,{"v":0.726061341,"d":"0.73"},{"$f":"VLOOKUP(A1707,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":0.51449924957483,"d":"0.51"}]
["05005","05","AR","005","Baxter","","2104009000","Wax Log; Total: All Combustor Types",null,264.24996210607196,"A","CEC Survey",2017,15,"I",90.75103417363566,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1708,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":0.243359375,"d":"0.24"}]
["05005","05","AR","005","Baxter","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",738.1121906925,"A","CEC Survey",2017,15,"I",1766.871825371468,"TON",8,{"v":2.3937713638272,"d":"2.39"},{"$f":"VLOOKUP(A1709,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":1.696266556,"d":"1.70"}]
["05005","05","AR","005","Baxter","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",976.2128973674999,"A","CEC Survey",2017,15,"I",2336.830478717103,"TON",8,{"v":2.3937713638272,"d":"2.39"},{"$f":"VLOOKUP(A1710,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":1.696266556,"d":"1.70"}]
["05005","05","AR","005","Baxter","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",666.68197869,"A","CEC Survey",2017,15,"I",1595.8842293677778,"TON",8,{"v":2.3937713638272,"d":"2.39"},{"$f":"VLOOKUP(A1711,cordwood_density!A:D,4,FALSE)","v":1.4112},{"v":1.696266556,"d":"1.70"}]
["05007","05","AR","007","Benton","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",372.6778922753988,"A","CEC Survey",2017,15,"I",1508.5331565962872,"TON",8,{"v":4.047820350667655,"d":"4.05"},{"$f":"VLOOKUP(A1712,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":2.811181575573064,"d":"2.81"}]
["05007","05","AR","007","Benton","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",30.217126400708008,"A","CEC Survey",2017,15,"I",122.31349918348275,"TON",8,{"v":4.0478203506676556,"d":"4.05"},{"$f":"VLOOKUP(A1713,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":2.8111815755730647,"d":"2.81"}]
["05007","05","AR","007","Benton","","2104008610","Hydronic heater: outdoor","Hydronic heater",362.6055168084961,"A","CEC Survey",2017,15,"I",1467.761990201793,"TON",8,{"v":4.0478203506676556,"d":"4.05"},{"$f":"VLOOKUP(A1714,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":2.8111815755730647,"d":"2.81"}]
["05007","05","AR","007","Benton","","2104008620","Hydronic heater: indoor","Hydronic heater",231.6646357387614,"A","CEC Survey",2017,15,"I",937.7368270733677,"TON",8,{"v":4.047820350667655,"d":"4.05"},{"$f":"VLOOKUP(A1715,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":2.811181575573064,"d":"2.81"}]
["05007","05","AR","007","Benton","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.07237546690267,"A","CEC Survey",2017,15,"I",40.77116639449425,"TON",8,{"v":4.047820350667655,"d":"4.05"},{"$f":"VLOOKUP(A1716,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":2.811181575573064,"d":"2.81"}]
["05007","05","AR","007","Benton","","2104008100","Fireplace: general","Fireplace: general",11023.989898872,"A","CEC Survey",2017,15,"I",6385.395080347343,"TON",8,{"v":0.5792272252535999,"d":"0.58"},{"$f":"VLOOKUP(A1717,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":0.40226906399999995,"d":"0.40"}]
["05007","05","AR","007","Benton","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1579.9582814101198,"A","CEC Survey",2017,15,"I",1735.6234533254578,"TON",8,{"v":1.0985248621732,"d":"1.10"},{"$f":"VLOOKUP(A1718,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":0.762917468,"d":"0.76"}]
["05007","05","AR","007","Benton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2089.6222431553197,"A","CEC Survey",2017,15,"I",2295.5019866562507,"TON",8,{"v":1.0985248621732,"d":"1.10"},{"$f":"VLOOKUP(A1719,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":0.762917468,"d":"0.76"}]
["05007","05","AR","007","Benton","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1427.05909288656,"A","CEC Survey",2017,15,"I",1567.65989332622,"TON",8,{"v":1.0985248621732,"d":"1.10"},{"$f":"VLOOKUP(A1720,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":0.762917468,"d":"0.76"}]
["05007","05","AR","007","Benton","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,12657.829710066,"A","CEC Survey",2017,15,"I",6139.944995587404,"TON",8,{"v":0.48507091154060006,"d":"0.49"},{"$f":"VLOOKUP(A1721,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":0.3368781940000001,"d":"0.34"}]
["05007","05","AR","007","Benton","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2687.002456992,"A","CEC Survey",2017,15,"I",1340.8349670109737,"TON",8,{"v":0.49900771900000007,"d":"0.50"},{"$f":"VLOOKUP(A1722,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":0.3465572046669908,"d":"0.35"}]
["05007","05","AR","007","Benton","","2104009000","Wax Log; Total: All Combustor Types",null,1305.6803486908675,"A","CEC Survey",2017,15,"I",448.40817005046875,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1723,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":0.2385087506076811,"d":"0.24"}]
["05007","05","AR","007","Benton","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",2364.63434788038,"A","CEC Survey",2017,15,"I",4723.894166673238,"TON",8,{"v":1.9977271204351996,"d":"2.00"},{"$f":"VLOOKUP(A1724,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":1.3874068479999997,"d":"1.39"}]
["05007","05","AR","007","Benton","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3127.41962139018,"A","CEC Survey",2017,15,"I",6247.730994632348,"TON",8,{"v":1.9977271204351998,"d":"2.00"},{"$f":"VLOOKUP(A1725,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":1.387406848,"d":"1.39"}]
["05007","05","AR","007","Benton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2135.79876582744,"A","CEC Survey",2017,15,"I",4266.743118285506,"TON",8,{"v":1.9977271204352,"d":"2.00"},{"$f":"VLOOKUP(A1726,cordwood_density!A:D,4,FALSE)","v":1.4399},{"v":1.3874068480000001,"d":"1.39"}]
["05009","05","AR","009","Boone","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",97.28205900351264,"A","CEC Survey",2017,15,"I",416.70786692034704,"TON",8,{"v":4.283501718495706,"d":"4.28"},{"$f":"VLOOKUP(A1727,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":2.933302553239544,"d":"2.93"}]
["05009","05","AR","009","Boone","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.887734513798323,"A","CEC Survey",2017,15,"I",33.787124344893,"TON",8,{"v":4.283501718495705,"d":"4.28"},{"$f":"VLOOKUP(A1728,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":2.9333025532395434,"d":"2.93"}]
["05009","05","AR","009","Boone","","2104008610","Hydronic heater: outdoor","Hydronic heater",94.65281416557987,"A","CEC Survey",2017,15,"I",405.445492138716,"TON",8,{"v":4.283501718495706,"d":"4.28"},{"$f":"VLOOKUP(A1729,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":2.933302553239544,"d":"2.93"}]
["05009","05","AR","009","Boone","","2104008620","Hydronic heater: indoor","Hydronic heater",60.47263127245381,"A","CEC Survey",2017,15,"I",259.03461997751305,"TON",8,{"v":4.283501718495706,"d":"4.28"},{"$f":"VLOOKUP(A1730,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":2.933302553239544,"d":"2.93"}]
["05009","05","AR","009","Boone","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.629244837932774,"A","CEC Survey",2017,15,"I",11.262374781631001,"TON",8,{"$f":"P1731/J1731","v":{"v":4.283501718495706,"d":"4.28"}},{"$f":"VLOOKUP(A1731,cordwood_density!A:D,4,FALSE)","v":1.4603},{"$f":"S1731/T1731","v":{"v":2.933302553239544,"d":"2.93"}}]
["05009","05","AR","009","Boone","","2104008100","Fireplace: general","Fireplace: general",1423.74608369,"A","CEC Survey",2017,15,"I",964.2573837930887,"TON",8,{"v":0.6772678041676999,"d":"0.68"},{"$f":"VLOOKUP(A1732,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":0.463786759,"d":"0.46"}]
["05009","05","AR","009","Boone","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",331.76956104911,"A","CEC Survey",2017,15,"I",367.96595188503676,"TON",8,{"v":1.1091009998671,"d":"1.11"},{"$f":"VLOOKUP(A1733,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":0.759502157,"d":"0.76"}]
["05009","05","AR","009","Boone","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",438.79200009720995,"A","CEC Survey",2017,15,"I",486.6646460415002,"TON",8,{"v":1.1091009998671,"d":"1.11"},{"$f":"VLOOKUP(A1734,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":0.759502157,"d":"0.76"}]
["05009","05","AR","009","Boone","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",299.66282933468005,"A","CEC Survey",2017,15,"I",332.3563436380977,"TON",8,{"v":1.1091009998670998,"d":"1.11"},{"$f":"VLOOKUP(A1735,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":0.7595021569999999,"d":"0.76"}]
["05009","05","AR","009","Boone","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2261.2112764030003,"A","CEC Survey",2017,15,"I",1107.5312810101009,"TON",8,{"v":0.48979557663089995,"d":"0.49"},{"$f":"VLOOKUP(A1736,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":0.335407503,"d":"0.34"}]
["05009","05","AR","009","Boone","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",556.738770889,"A","CEC Survey",2017,15,"I",337.5044896563762,"TON",8,{"v":0.606216968,"d":"0.61"},{"$f":"VLOOKUP(A1737,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":0.4151318003150038,"d":"0.42"}]
["05009","05","AR","009","Boone","","2104009000","Wax Log; Total: All Combustor Types",null,213.82156679384136,"A","CEC Survey",2017,15,"I",73.43247340705045,"TON",8,{"v":0.34342875000000006,"d":"0.34"},{"$f":"VLOOKUP(A1738,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":0.23517684722317336,"d":"0.24"}]
["05009","05","AR","009","Boone","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",571.16002618129,"A","CEC Survey",2017,15,"I",1356.7829438772683,"TON",8,{"v":2.3754865216120993,"d":"2.38"},{"$f":"VLOOKUP(A1739,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":1.6267113069999997,"d":"1.63"}]
["05009","05","AR","009","Boone","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",755.40519591719,"A","CEC Survey",2017,15,"I",1794.4548612570322,"TON",8,{"v":2.3754865216120997,"d":"2.38"},{"$f":"VLOOKUP(A1740,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":1.6267113069999999,"d":"1.63"}]
["05009","05","AR","009","Boone","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",515.8864752605201,"A","CEC Survey",2017,15,"I",1225.4813686633393,"TON",8,{"v":2.3754865216120993,"d":"2.38"},{"$f":"VLOOKUP(A1741,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":1.6267113069999997,"d":"1.63"}]
["05011","05","AR","011","Bradley","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",22.289106566726083,"A","CEC Survey",2017,15,"I",81.23303333702741,"TON",8,{"v":3.6445172485421544,"d":"3.64"},{"$f":"VLOOKUP(A1742,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":2.750371480297453,"d":"2.75"}]
["05011","05","AR","011","Bradley","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.8072248567615743,"A","CEC Survey",2017,15,"I",6.586462162461682,"TON",8,{"v":3.644517248542155,"d":"3.64"},{"$f":"VLOOKUP(A1743,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":2.750371480297453,"d":"2.75"}]
["05011","05","AR","011","Bradley","","2104008610","Hydronic heater: outdoor","Hydronic heater",21.68669828113889,"A","CEC Survey",2017,15,"I",79.03754594954019,"TON",8,{"v":3.644517248542155,"d":"3.64"},{"$f":"VLOOKUP(A1744,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":2.750371480297453,"d":"2.75"}]
["05011","05","AR","011","Bradley","","2104008620","Hydronic heater: indoor","Hydronic heater",13.855390568505404,"A","CEC Survey",2017,15,"I",50.49620991220623,"TON",8,{"v":3.6445172485421544,"d":"3.64"},{"$f":"VLOOKUP(A1745,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":2.750371480297453,"d":"2.75"}]
["05011","05","AR","011","Bradley","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.6024082855871915,"A","CEC Survey",2017,15,"I",2.1954873874872276,"TON",8,{"v":3.6445172485421544,"d":"3.64"},{"$f":"VLOOKUP(A1746,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":2.750371480297453,"d":"2.75"}]
["05011","05","AR","011","Bradley","","2104008100","Fireplace: general","Fireplace: general",631.21032372,"A","CEC Survey",2017,15,"I",368.80036045890785,"TON",8,{"v":0.5842749185175,"d":"0.58"},{"$f":"VLOOKUP(A1747,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":0.440928925,"d":"0.44"}]
["05011","05","AR","011","Bradley","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",125.04769548660002,"A","CEC Survey",2017,15,"I",188.43551174233832,"TON",8,{"v":1.5069091118319,"d":"1.51"},{"$f":"VLOOKUP(A1748,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":1.137204069,"d":"1.14"}]
["05011","05","AR","011","Bradley","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",165.3856617726,"A","CEC Survey",2017,15,"I",249.22116069147972,"TON",8,{"v":1.5069091118319002,"d":"1.51"},{"$f":"VLOOKUP(A1749,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":1.1372040690000003,"d":"1.14"}]
["05011","05","AR","011","Bradley","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",112.94630560080003,"A","CEC Survey",2017,15,"I",170.19981705759594,"TON",8,{"v":1.5069091118319,"d":"1.51"},{"$f":"VLOOKUP(A1750,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":1.137204069,"d":"1.14"}]
["05011","05","AR","011","Bradley","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,670.2365010359999,"A","CEC Survey",2017,15,"I",296.17567462982663,"TON",8,{"v":0.4418972618948999,"d":"0.44"},{"$f":"VLOOKUP(A1751,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":0.333482199,"d":"0.33"}]
["05011","05","AR","011","Bradley","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",144.640761744,"A","CEC Survey",2017,15,"I",86.08713684663485,"TON",8,{"v":0.595178951,"d":"0.60"},{"$f":"VLOOKUP(A1752,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":0.4491577624330239,"d":"0.45"}]
["05011","05","AR","011","Bradley","","2104009000","Wax Log; Total: All Combustor Types",null,65.58133095860009,"A","CEC Survey",2017,15,"I",15.354707854398244,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1753,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":0.17669028752546978,"d":"0.18"}]
["05011","05","AR","011","Bradley","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",151.89167640576,"A","CEC Survey",2017,15,"I",330.24139025372483,"TON",8,{"v":2.1741901733412003,"d":"2.17"},{"$f":"VLOOKUP(A1754,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":1.6407744120000003,"d":"1.64"}]
["05011","05","AR","011","Bradley","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",200.88899137535998,"A","CEC Survey",2017,15,"I",436.7708709807328,"TON",8,{"v":2.1741901733412003,"d":"2.17"},{"$f":"VLOOKUP(A1755,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":1.6407744120000003,"d":"1.64"}]
["05011","05","AR","011","Bradley","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",137.19248191488,"A","CEC Survey",2017,15,"I",298.2825460356225,"TON",8,{"v":2.174190173341201,"d":"2.17"},{"$f":"VLOOKUP(A1756,cordwood_density!A:D,4,FALSE)","v":1.3251},{"v":1.6407744120000007,"d":"1.64"}]
["05013","05","AR","013","Calhoun","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",15.850026939870572,"A","CEC Survey",2017,15,"I",57.26880966225576,"TON",8,{"v":3.613167969967085,"d":"3.61"},{"$f":"VLOOKUP(A1757,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":2.777650653418731,"d":"2.78"}]
["05013","05","AR","013","Calhoun","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.2851373194489653,"A","CEC Survey",2017,15,"I",4.643416999642359,"TON",8,{"v":3.613167969967085,"d":"3.61"},{"$f":"VLOOKUP(A1758,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":2.777650653418731,"d":"2.78"}]
["05013","05","AR","013","Calhoun","","2104008610","Hydronic heater: outdoor","Hydronic heater",15.421647833387583,"A","CEC Survey",2017,15,"I",55.72100399570831,"TON",8,{"v":3.613167969967085,"d":"3.61"},{"$f":"VLOOKUP(A1759,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":2.777650653418731,"d":"2.78"}]
["05013","05","AR","013","Calhoun","","2104008620","Hydronic heater: indoor","Hydronic heater",9.852719449108735,"A","CEC Survey",2017,15,"I",35.59953033059142,"TON",8,{"v":3.6131679699670847,"d":"3.61"},{"$f":"VLOOKUP(A1760,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":2.7776506534187306,"d":"2.78"}]
["05013","05","AR","013","Calhoun","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.42837910648298844,"A","CEC Survey",2017,15,"I",1.547805666547453,"TON",8,{"v":3.613167969967085,"d":"3.61"},{"$f":"VLOOKUP(A1761,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":2.777650653418731,"d":"2.78"}]
["05013","05","AR","013","Calhoun","","2104008100","Fireplace: general","Fireplace: general",314.09444205,"A","CEC Survey",2017,15,"I",202.01536687304798,"TON",8,{"v":0.6431675949263999,"d":"0.64"},{"$f":"VLOOKUP(A1762,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":0.4944400329999999,"d":"0.49"}]
["05013","05","AR","013","Calhoun","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",59.8518620928,"A","CEC Survey",2017,15,"I",89.53474372762052,"TON",8,{"v":1.4959391503776,"d":"1.50"},{"$f":"VLOOKUP(A1763,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":1.150014722,"d":"1.15"}]
["05013","05","AR","013","Calhoun","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",79.1589143808,"A","CEC Survey",2017,15,"I",118.41691912362712,"TON",8,{"v":1.4959391503775998,"d":"1.50"},{"$f":"VLOOKUP(A1764,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":1.1500147219999999,"d":"1.15"}]
["05013","05","AR","013","Calhoun","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",54.0597464064,"A","CEC Survey",2017,15,"I",80.87009110881854,"TON",8,{"v":1.4959391503776,"d":"1.50"},{"$f":"VLOOKUP(A1765,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":1.150014722,"d":"1.15"}]
["05013","05","AR","013","Calhoun","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,342.584102592,"A","CEC Survey",2017,15,"I",149.74193448510545,"TON",8,{"v":0.43709539745759995,"d":"0.44"},{"$f":"VLOOKUP(A1766,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":0.336020447,"d":"0.34"}]
["05013","05","AR","013","Calhoun","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",86.277530475,"A","CEC Survey",2017,15,"I",59.55260615507404,"TON",8,{"v":0.690244677,"d":"0.69"},{"$f":"VLOOKUP(A1767,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":0.5306309017527676,"d":"0.53"}]
["05013","05","AR","013","Calhoun","","2104009000","Wax Log; Total: All Combustor Types",null,29.602085656082963,"A","CEC Survey",2017,15,"I",6.930804399455713,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A1768,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":0.17999100553505537,"d":"0.18"}]
["05013","05","AR","013","Calhoun","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",88.95832206192,"A","CEC Survey",2017,15,"I",214.99274460293222,"TON",8,{"v":2.416780573416,"d":"2.42"},{"$f":"VLOOKUP(A1769,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":1.8579186450000003,"d":"1.86"}]
["05013","05","AR","013","Calhoun","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",117.65455498512,"A","CEC Survey",2017,15,"I",284.3452428619426,"TON",8,{"v":2.4167805734159997,"d":"2.42"},{"$f":"VLOOKUP(A1770,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":1.8579186449999998,"d":"1.86"}]
["05013","05","AR","013","Calhoun","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",80.34945218496001,"A","CEC Survey",2017,15,"I",194.18699512522912,"TON",8,{"v":2.4167805734159997,"d":"2.42"},{"$f":"VLOOKUP(A1771,cordwood_density!A:D,4,FALSE)","v":1.3008},{"v":1.8579186449999998,"d":"1.86"}]
["05015","05","AR","015","Carroll","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",85.37497411411894,"A","CEC Survey",2017,15,"I",366.4752150607875,"TON",8,{"v":4.292536763418841,"d":"4.29"},{"$f":"VLOOKUP(A1772,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":2.976174695568773,"d":"2.98"}]
["05015","05","AR","015","Carroll","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.922295198442076,"A","CEC Survey",2017,15,"I",29.714206626550336,"TON",8,{"v":4.292536763418841,"d":"4.29"},{"$f":"VLOOKUP(A1773,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":2.976174695568773,"d":"2.98"}]
["05015","05","AR","015","Carroll","","2104008610","Hydronic heater: outdoor","Hydronic heater",83.06754238130492,"A","CEC Survey",2017,15,"I",356.57047951860403,"TON",8,{"v":4.292536763418841,"d":"4.29"},{"$f":"VLOOKUP(A1774,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":2.976174695568773,"d":"2.98"}]
["05015","05","AR","015","Carroll","","2104008620","Hydronic heater: indoor","Hydronic heater",53.07092985472259,"A","CEC Survey",2017,15,"I",227.80891747021926,"TON",8,{"v":4.292536763418841,"d":"4.29"},{"$f":"VLOOKUP(A1775,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":2.976174695568773,"d":"2.98"}]
["05015","05","AR","015","Carroll","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.3074317328140257,"A","CEC Survey",2017,15,"I",9.904735542183445,"TON",8,{"v":4.292536763418841,"d":"4.29"},{"$f":"VLOOKUP(A1776,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":2.976174695568773,"d":"2.98"}]
["05015","05","AR","015","Carroll","","2104008100","Fireplace: general","Fireplace: general",1011.014122176,"A","CEC Survey",2017,15,"I",702.2287773364628,"TON",8,{"v":0.6945786037341,"d":"0.69"},{"$f":"VLOOKUP(A1777,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":0.481577067,"d":"0.48"}]
["05015","05","AR","015","Carroll","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",264.49792528544003,"A","CEC Survey",2017,15,"I",310.33588281823404,"TON",8,{"v":1.1733017659148999,"d":"1.17"},{"$f":"VLOOKUP(A1778,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":0.813493563,"d":"0.81"}]
["05015","05","AR","015","Carroll","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",349.81983666784,"A","CEC Survey",2017,15,"I",410.44423211443853,"TON",8,{"v":1.1733017659149,"d":"1.17"},{"$f":"VLOOKUP(A1779,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":0.8134935630000001,"d":"0.81"}]
["05015","05","AR","015","Carroll","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",238.90135187072002,"A","CEC Survey",2017,15,"I",280.3033780293727,"TON",8,{"v":1.1733017659149,"d":"1.17"},{"$f":"VLOOKUP(A1780,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":0.8134935630000001,"d":"0.81"}]
["05015","05","AR","015","Carroll","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1671.994850688,"A","CEC Survey",2017,15,"I",804.9690876371357,"TON",8,{"v":0.4814423246015999,"d":"0.48"},{"$f":"VLOOKUP(A1781,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":0.333801792,"d":"0.33"}]
["05015","05","AR","015","Carroll","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",425.093618512,"A","CEC Survey",2017,15,"I",304.99832590991645,"TON",8,{"v":0.717485073,"d":"0.72"},{"$f":"VLOOKUP(A1782,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":0.49745897039450876,"d":"0.50"}]
["05015","05","AR","015","Carroll","","2104009000","Wax Log; Total: All Combustor Types",null,155.57971461751123,"A","CEC Survey",2017,15,"I",53.43054691644861,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1783,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":0.23811186992997296,"d":"0.24"}]
["05015","05","AR","015","Carroll","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",474.04069262352,"A","CEC Survey",2017,15,"I",1180.5786767037832,"TON",8,{"v":2.4904585093106997,"d":"2.49"},{"$f":"VLOOKUP(A1784,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":1.7267271089999998,"d":"1.73"}]
["05015","05","AR","015","Carroll","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",626.9570450827199,"A","CEC Survey",2017,15,"I",1561.410507898552,"TON",8,{"v":2.4904585093107,"d":"2.49"},{"$f":"VLOOKUP(A1785,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":1.7267271090000003,"d":"1.73"}]
["05015","05","AR","015","Carroll","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",428.16578688576004,"A","CEC Survey",2017,15,"I",1066.3291273453528,"TON",8,{"v":2.4904585093107,"d":"2.49"},{"$f":"VLOOKUP(A1786,cordwood_density!A:D,4,FALSE)","v":1.4423},{"v":1.7267271090000003,"d":"1.73"}]
["05017","05","AR","017","Chicot","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",14.024870515863135,"A","CEC Survey",2017,15,"I",48.263274415351866,"TON",8,{"v":3.4412634584228523,"d":"3.44"},{"$f":"VLOOKUP(A1787,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":2.695225139742209,"d":"2.70"}]
["05017","05","AR","017","Chicot","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.1371516634483623,"A","CEC Survey",2017,15,"I",3.9132384661096102,"TON",8,{"v":3.441263458422852,"d":"3.44"},{"$f":"VLOOKUP(A1788,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":2.6952251397422087,"d":"2.70"}]
["05017","05","AR","017","Chicot","","2104008610","Hydronic heater: outdoor","Hydronic heater",13.645819961380347,"A","CEC Survey",2017,15,"I",46.958861593315326,"TON",8,{"v":3.4412634584228523,"d":"3.44"},{"$f":"VLOOKUP(A1789,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":2.695225139742209,"d":"2.70"}]
["05017","05","AR","017","Chicot","","2104008620","Hydronic heater: indoor","Hydronic heater",8.718162753104112,"A","CEC Survey",2017,15,"I",30.00149490684035,"TON",8,{"v":3.441263458422852,"d":"3.44"},{"$f":"VLOOKUP(A1790,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":2.6952251397422087,"d":"2.70"}]
["05017","05","AR","017","Chicot","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.37905055448278746,"A","CEC Survey",2017,15,"I",1.304412822036537,"TON",8,{"v":3.4412634584228523,"d":"3.44"},{"$f":"VLOOKUP(A1791,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":2.695225139742209,"d":"2.70"}]
["05017","05","AR","017","Chicot","","2104008100","Fireplace: general","Fireplace: general",273.953113995,"A","CEC Survey",2017,15,"I",177.914447993144,"TON",8,{"v":0.6494339319552,"d":"0.65"},{"$f":"VLOOKUP(A1792,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":0.5086418640000001,"d":"0.51"}]
["05017","05","AR","017","Chicot","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",78.82629784557,"A","CEC Survey",2017,15,"I",55.41943171772284,"TON",8,{"v":0.7030576499519999,"d":"0.70"},{"$f":"VLOOKUP(A1793,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":0.55064039,"d":"0.55"}]
["05017","05","AR","017","Chicot","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",104.25413586027,"A","CEC Survey",2017,15,"I",73.29666775569794,"TON",8,{"v":0.7030576499519998,"d":"0.70"},{"$f":"VLOOKUP(A1794,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":0.5506403899999999,"d":"0.55"}]
["05017","05","AR","017","Chicot","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",71.19794644116001,"A","CEC Survey",2017,15,"I",50.05626090633031,"TON",8,{"$f":"P1795/J1795","v":{"v":0.7030576499519998,"d":"0.70"}},{"$f":"VLOOKUP(A1795,cordwood_density!A:D,4,FALSE)","v":1.2768},{"$f":"S1795/T1795","v":{"v":0.5506403899999999,"d":"0.55"}}]
["05017","05","AR","017","Chicot","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,584.280896727,"A","CEC Survey",2017,15,"I",249.69081687799658,"TON",8,{"v":0.427347219936,"d":"0.43"},{"$f":"VLOOKUP(A1796,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":0.33470177,"d":"0.33"}]
["05017","05","AR","017","Chicot","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",144.91713201899998,"A","CEC Survey",2017,15,"I",42.23898183294759,"TON",8,{"v":0.291469899,"d":"0.29"},{"$f":"VLOOKUP(A1797,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":0.2282815625,"d":"0.23"}]
["05017","05","AR","017","Chicot","","2104009000","Wax Log; Total: All Combustor Types",null,62.091128719673286,"A","CEC Survey",2017,15,"I",14.537538776733161,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1798,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":0.18337429511278194,"d":"0.18"}]
["05017","05","AR","017","Chicot","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",121.46211165461999,"A","CEC Survey",2017,15,"I",229.5558251728968,"TON",8,{"v":1.8899377101696,"d":"1.89"},{"$f":"VLOOKUP(A1799,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":1.480214372,"d":"1.48"}]
["05017","05","AR","017","Chicot","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",160.64343799481998,"A","CEC Survey",2017,15,"I",303.60609135770216,"TON",8,{"v":1.8899377101695998,"d":"1.89"},{"$f":"VLOOKUP(A1800,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":1.4802143719999998,"d":"1.48"}]
["05017","05","AR","017","Chicot","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",109.70771375256,"A","CEC Survey",2017,15,"I",207.34074531745517,"TON",8,{"v":1.8899377101696,"d":"1.89"},{"$f":"VLOOKUP(A1801,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":1.480214372,"d":"1.48"}]
["05019","05","AR","019","Clark","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",42.977827502386035,"A","CEC Survey",2017,15,"I",152.21794460131153,"TON",8,{"v":3.5417784808424932,"d":"3.54"},{"$f":"VLOOKUP(A1802,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":2.6845891615572604,"d":"2.68"}]
["05019","05","AR","019","Clark","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.4846887164096785,"A","CEC Survey",2017,15,"I",12.341995508214447,"TON",8,{"v":3.541778480842493,"d":"3.54"},{"$f":"VLOOKUP(A1803,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":2.68458916155726,"d":"2.68"}]
["05019","05","AR","019","Clark","","2104008610","Hydronic heater: outdoor","Hydronic heater",41.81626459691614,"A","CEC Survey",2017,15,"I",148.10394609857337,"TON",8,{"v":3.541778480842493,"d":"3.54"},{"$f":"VLOOKUP(A1804,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":2.68458916155726,"d":"2.68"}]
["05019","05","AR","019","Clark","","2104008620","Hydronic heater: indoor","Hydronic heater",26.715946825807535,"A","CEC Survey",2017,15,"I",94.62196556297744,"TON",8,{"v":3.5417784808424932,"d":"3.54"},{"$f":"VLOOKUP(A1805,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":2.6845891615572604,"d":"2.68"}]
["05019","05","AR","019","Clark","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.1615629054698928,"A","CEC Survey",2017,15,"I",4.113998502738149,"TON",8,{"v":3.5417784808424932,"d":"3.54"},{"$f":"VLOOKUP(A1806,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":2.6845891615572604,"d":"2.68"}]
["05019","05","AR","019","Clark","","2104008100","Fireplace: general","Fireplace: general",1276.5649050000002,"A","CEC Survey",2017,15,"I",739.5253661543844,"TON",8,{"v":0.579308864953,"d":"0.58"},{"$f":"VLOOKUP(A1807,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":0.4391032100000001,"d":"0.44"}]
["05019","05","AR","019","Clark","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",209.0883753,"A","CEC Survey",2017,15,"I",304.6554655600772,"TON",8,{"v":1.4570655356757998,"d":"1.46"},{"$f":"VLOOKUP(A1808,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":1.1044232059999999,"d":"1.10"}]
["05019","05","AR","019","Clark","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",276.5362383,"A","CEC Survey",2017,15,"I",402.9314221923601,"TON",8,{"v":1.4570655356757998,"d":"1.46"},{"$f":"VLOOKUP(A1809,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":1.1044232059999999,"d":"1.10"}]
["05019","05","AR","019","Clark","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",188.8540164,"A","CEC Survey",2017,15,"I",275.17267857039235,"TON",8,{"v":1.4570655356758002,"d":"1.46"},{"$f":"VLOOKUP(A1810,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":1.1044232060000003,"d":"1.10"}]
["05019","05","AR","019","Clark","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1243.78284366,"A","CEC Survey",2017,15,"I",546.8084325545484,"TON",8,{"v":0.43963336151629995,"d":"0.44"},{"$f":"VLOOKUP(A1811,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":0.33323229099999996,"d":"0.33"}]
["05019","05","AR","019","Clark","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",278.06126922,"A","CEC Survey",2017,15,"I",157.15757971730957,"TON",8,{"v":0.565190471,"d":"0.57"},{"$f":"VLOOKUP(A1812,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":0.428401782005609,"d":"0.43"}]
["05019","05","AR","019","Clark","","2104009000","Wax Log; Total: All Combustor Types",null,126.68141459808429,"A","CEC Survey",2017,15,"I",29.660210967103048,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1813,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":0.17746706586826347,"d":"0.18"}]
["05019","05","AR","019","Clark","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",269.4806548686,"A","CEC Survey",2017,15,"I",596.6761880693692,"TON",8,{"v":2.2141707662106995,"d":"2.21"},{"$f":"VLOOKUP(A1814,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":1.6782920989999996,"d":"1.68"}]
["05019","05","AR","019","Clark","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",356.4098983746,"A","CEC Survey",2017,15,"I",789.1523777691657,"TON",8,{"v":2.2141707662106995,"d":"2.21"},{"$f":"VLOOKUP(A1815,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":1.6782920989999996,"d":"1.68"}]
["05019","05","AR","019","Clark","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",243.40188181680003,"A","CEC Survey",2017,15,"I",538.9333311594304,"TON",8,{"v":2.2141707662107,"d":"2.21"},{"$f":"VLOOKUP(A1816,cordwood_density!A:D,4,FALSE)","v":1.3193},{"v":1.678292099,"d":"1.68"}]
["05021","05","AR","021","Clay","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",29.120870707497883,"A","CEC Survey",2017,15,"I",110.36665217380845,"TON",8,{"v":3.789950282818702,"d":"3.79"},{"$f":"VLOOKUP(A1817,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":2.730315022562281,"d":"2.73"}]
["05021","05","AR","021","Clay","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.3611516789863147,"A","CEC Survey",2017,15,"I",8.948647473552036,"TON",8,{"v":3.789950282818702,"d":"3.79"},{"$f":"VLOOKUP(A1818,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":2.730315022562281,"d":"2.73"}]
["05021","05","AR","021","Clay","","2104008610","Hydronic heater: outdoor","Hydronic heater",28.333820147835777,"A","CEC Survey",2017,15,"I",107.38376968262443,"TON",8,{"v":3.789950282818702,"d":"3.79"},{"$f":"VLOOKUP(A1819,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":2.730315022562281,"d":"2.73"}]
["05021","05","AR","021","Clay","","2104008620","Hydronic heater: indoor","Hydronic heater",18.102162872228416,"A","CEC Survey",2017,15,"I",68.60629729723229,"TON",8,{"v":3.789950282818702,"d":"3.79"},{"$f":"VLOOKUP(A1820,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":2.730315022562281,"d":"2.73"}]
["05021","05","AR","021","Clay","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7870505596621049,"A","CEC Survey",2017,15,"I",2.982882491184012,"TON",8,{"v":3.789950282818702,"d":"3.79"},{"$f":"VLOOKUP(A1821,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":2.730315022562281,"d":"2.73"}]
["05021","05","AR","021","Clay","","2104008100","Fireplace: general","Fireplace: general",553.608845236,"A","CEC Survey",2017,15,"I",382.7416308709106,"TON",8,{"v":0.6913575065943,"d":"0.69"},{"$f":"VLOOKUP(A1822,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":0.498060303,"d":"0.50"}]
["05021","05","AR","021","Clay","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",109.83082054252,"A","CEC Survey",2017,15,"I",88.51566437954754,"TON",8,{"v":0.8059273703165999,"d":"0.81"},{"$f":"VLOOKUP(A1823,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":0.5805974859999999,"d":"0.58"}]
["05021","05","AR","021","Clay","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",145.26011749172,"A","CEC Survey",2017,15,"I",117.06910450198224,"TON",8,{"v":0.8059273703166,"d":"0.81"},{"$f":"VLOOKUP(A1824,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":0.580597486,"d":"0.58"}]
["05021","05","AR","021","Clay","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",99.20203145776001,"A","CEC Survey",2017,15,"I",79.94963234281715,"TON",8,{"v":0.8059273703166,"d":"0.81"},{"$f":"VLOOKUP(A1825,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":0.580597486,"d":"0.58"}]
["05021","05","AR","021","Clay","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,964.993613736,"A","CEC Survey",2017,15,"I",448.12345200985715,"TON",8,{"v":0.46437970742099993,"d":"0.46"},{"$f":"VLOOKUP(A1826,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":0.33454341,"d":"0.33"}]
["05021","05","AR","021","Clay","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",244.638553132,"A","CEC Survey",2017,15,"I",85.09045383308188,"TON",8,{"v":0.347821113,"d":"0.35"},{"$f":"VLOOKUP(A1827,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":0.25057352712340614,"d":"0.25"}]
["05021","05","AR","021","Clay","","2104009000","Wax Log; Total: All Combustor Types",null,92.325185151529,"A","CEC Survey",2017,15,"I",31.707122930108167,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1828,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":0.24740922844175495,"d":"0.25"}]
["05021","05","AR","021","Clay","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",193.31363503107997,"A","CEC Survey",2017,15,"I",408.29025952697623,"TON",8,{"v":2.1120613631901,"d":"2.11"},{"$f":"VLOOKUP(A1829,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":1.521548421,"d":"1.52"}]
["05021","05","AR","021","Clay","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",255.67287213787995,"A","CEC Survey",2017,15,"I",539.9967948582589,"TON",8,{"v":2.1120613631901,"d":"2.11"},{"$f":"VLOOKUP(A1830,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":1.521548421,"d":"1.52"}]
["05021","05","AR","021","Clay","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",174.60586389904,"A","CEC Survey",2017,15,"I",368.7782989275915,"TON",8,{"v":2.1120613631901,"d":"2.11"},{"$f":"VLOOKUP(A1831,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":1.521548421,"d":"1.52"}]
["05023","05","AR","023","Cleburne","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",88.15259719022812,"A","CEC Survey",2017,15,"I",355.3560341293189,"TON",8,{"v":4.031146505672221,"d":"4.03"},{"$f":"VLOOKUP(A1832,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":3.0198116006234335,"d":"3.02"}]
["05023","05","AR","023","Cleburne","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.147507880288766,"A","CEC Survey",2017,15,"I",28.812651415890723,"TON",8,{"v":4.031146505672221,"d":"4.03"},{"$f":"VLOOKUP(A1833,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":3.0198116006234335,"d":"3.02"}]
["05023","05","AR","023","Cleburne","","2104008610","Hydronic heater: outdoor","Hydronic heater",85.7700945634652,"A","CEC Survey",2017,15,"I",345.75181699068867,"TON",8,{"v":4.031146505672221,"d":"4.03"},{"$f":"VLOOKUP(A1834,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":3.0198116006234335,"d":"3.02"}]
["05023","05","AR","023","Cleburne","","2104008620","Hydronic heater: indoor","Hydronic heater",54.79756041554721,"A","CEC Survey",2017,15,"I",220.89699418849557,"TON",8,{"v":4.031146505672221,"d":"4.03"},{"$f":"VLOOKUP(A1835,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":3.0198116006234335,"d":"3.02"}]
["05023","05","AR","023","Cleburne","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.382502626762922,"A","CEC Survey",2017,15,"I",9.604217138630242,"TON",8,{"v":4.031146505672221,"d":"4.03"},{"$f":"VLOOKUP(A1836,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":3.0198116006234335,"d":"3.02"}]
["05023","05","AR","023","Cleburne","","2104008100","Fireplace: general","Fireplace: general",1061.796141688,"A","CEC Survey",2017,15,"I",661.1630452619453,"TON",8,{"v":0.6226836012145,"d":"0.62"},{"$f":"VLOOKUP(A1837,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":0.466464605,"d":"0.47"}]
["05023","05","AR","023","Cleburne","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",300.43863775814003,"A","CEC Survey",2017,15,"I",359.97797195232863,"TON",8,{"v":1.1981746909733997,"d":"1.20"},{"$f":"VLOOKUP(A1838,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":0.8975763659999998,"d":"0.90"}]
["05023","05","AR","023","Cleburne","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",397.35432735754,"A","CEC Survey",2017,15,"I",476.09989838856364,"TON",8,{"v":1.1981746909734,"d":"1.20"},{"$f":"VLOOKUP(A1839,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":0.8975763659999999,"d":"0.90"}]
["05023","05","AR","023","Cleburne","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",271.36393087832005,"A","CEC Survey",2017,15,"I",325.14139402145815,"TON",8,{"v":1.1981746909734,"d":"1.20"},{"$f":"VLOOKUP(A1840,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":0.8975763659999999,"d":"0.90"}]
["05023","05","AR","023","Cleburne","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1668.8877942220001,"A","CEC Survey",2017,15,"I",746.4862332598932,"TON",8,{"v":0.4472956395537,"d":"0.45"},{"$f":"VLOOKUP(A1841,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":0.335078013,"d":"0.34"}]
["05023","05","AR","023","Cleburne","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",413.56063745,"A","CEC Survey",2017,15,"I",335.7350953061965,"TON",8,{"v":0.811815886,"d":"0.81"},{"$f":"VLOOKUP(A1842,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":0.6081473413738857,"d":"0.61"}]
["05023","05","AR","023","Cleburne","","2104009000","Wax Log; Total: All Combustor Types",null,152.90820179265367,"A","CEC Survey",2017,15,"I",52.51307260639881,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1843,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":0.2572692711064499,"d":"0.26"}]
["05023","05","AR","023","Cleburne","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",501.46266236686,"A","CEC Survey",2017,15,"I",1185.1226912025295,"TON",8,{"v":2.363331869234,"d":"2.36"},{"$f":"VLOOKUP(A1844,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":1.77041866,"d":"1.77"}]
["05023","05","AR","023","Cleburne","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",663.2248115174599,"A","CEC Survey",2017,15,"I",1567.420333525926,"TON",8,{"v":2.3633318692340004,"d":"2.36"},{"$f":"VLOOKUP(A1845,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":1.7704186600000003,"d":"1.77"}]
["05023","05","AR","023","Cleburne","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",452.93401762168,"A","CEC Survey",2017,15,"I",1070.4333985055107,"TON",8,{"v":2.3633318692340004,"d":"2.36"},{"$f":"VLOOKUP(A1846,cordwood_density!A:D,4,FALSE)","v":1.3349},{"v":1.7704186600000003,"d":"1.77"}]
["05025","05","AR","025","Cleveland","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",26.77856758863825,"A","CEC Survey",2017,15,"I",102.44124161507173,"TON",8,{"v":3.8254937003626748,"d":"3.83"},{"$f":"VLOOKUP(A1847,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":2.887382972573534,"d":"2.89"}]
["05025","05","AR","025","Cleveland","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.1712352098895877,"A","CEC Survey",2017,15,"I",8.306046617438248,"TON",8,{"v":3.825493700362675,"d":"3.83"},{"$f":"VLOOKUP(A1848,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":2.8873829725735343,"d":"2.89"}]
["05025","05","AR","025","Cleveland","","2104008610","Hydronic heater: outdoor","Hydronic heater",26.054822518675053,"A","CEC Survey",2017,15,"I",99.67255940925898,"TON",8,{"v":3.825493700362675,"d":"3.83"},{"$f":"VLOOKUP(A1849,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":2.8873829725735343,"d":"2.89"}]
["05025","05","AR","025","Cleveland","","2104008620","Hydronic heater: indoor","Hydronic heater",16.64613660915351,"A","CEC Survey",2017,15,"I",63.67969073369324,"TON",8,{"v":3.8254937003626748,"d":"3.83"},{"$f":"VLOOKUP(A1850,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":2.887382972573534,"d":"2.89"}]
["05025","05","AR","025","Cleveland","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.723745069963196,"A","CEC Survey",2017,15,"I",2.7686822058127496,"TON",8,{"v":3.8254937003626748,"d":"3.83"},{"$f":"VLOOKUP(A1851,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":2.887382972573534,"d":"2.89"}]
["05025","05","AR","025","Cleveland","","2104008100","Fireplace: general","Fireplace: general",403.536839644,"A","CEC Survey",2017,15,"I",260.130581414318,"TON",8,{"v":0.6446266012387,"d":"0.64"},{"$f":"VLOOKUP(A1852,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":0.486547363,"d":"0.49"}]
["05025","05","AR","025","Cleveland","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",112.5806589166,"A","CEC Survey",2017,15,"I",174.3931448976937,"TON",8,{"v":1.5490506679915999,"d":"1.55"},{"$f":"VLOOKUP(A1853,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":1.169183084,"d":"1.17"}]
["05025","05","AR","025","Cleveland","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",148.89700050259998,"A","CEC Survey",2017,15,"I",230.6489980904981,"TON",8,{"v":1.5490506679916,"d":"1.55"},{"$f":"VLOOKUP(A1854,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":1.1691830840000002,"d":"1.17"}]
["05025","05","AR","025","Cleveland","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",101.6857564408,"A","CEC Survey",2017,15,"I",157.5163889398524,"TON",8,{"v":1.5490506679916,"d":"1.55"},{"$f":"VLOOKUP(A1855,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":1.1691830840000002,"d":"1.17"}]
["05025","05","AR","025","Cleveland","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,539.048665096,"A","CEC Survey",2017,15,"I",239.6963672354086,"TON",8,{"v":0.4446655427534,"d":"0.44"},{"$f":"VLOOKUP(A1856,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":0.335621966,"d":"0.34"}]
["05025","05","AR","025","Cleveland","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",135.422901948,"A","CEC Survey",2017,15,"I",110.37816626028979,"TON",8,{"v":0.815062775,"d":"0.82"},{"$f":"VLOOKUP(A1857,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":0.6151881462751906,"d":"0.62"}]
["05025","05","AR","025","Cleveland","","2104009000","Wax Log; Total: All Combustor Types",null,47.282904405543476,"A","CEC Survey",2017,15,"I",11.070455159150026,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A1858,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":0.1767169597705487,"d":"0.18"}]
["05025","05","AR","025","Cleveland","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",164.11714036944,"A","CEC Survey",2017,15,"I",407.46710521883034,"TON",8,{"$f":"P1859/J1859","v":{"v":2.4827821414728,"d":"2.48"}},{"$f":"VLOOKUP(A1859,cordwood_density!A:D,4,FALSE)","v":1.3249},{"$f":"S1859/T1859","v":{"v":1.873939272,"d":"1.87"}}]
["05025","05","AR","025","Cleveland","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",217.05815339184,"A","CEC Survey",2017,15,"I",538.908106902324,"TON",8,{"v":2.4827821414728,"d":"2.48"},{"$f":"VLOOKUP(A1860,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":1.873939272,"d":"1.87"}]
["05025","05","AR","025","Cleveland","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",148.23483646272,"A","CEC Survey",2017,15,"I",368.0348047137823,"TON",8,{"v":2.4827821414728,"d":"2.48"},{"$f":"VLOOKUP(A1861,cordwood_density!A:D,4,FALSE)","v":1.3249},{"v":1.873939272,"d":"1.87"}]
["05027","05","AR","027","Columbia","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",51.17242265801734,"A","CEC Survey",2017,15,"I",179.73247785595933,"TON",8,{"v":3.5122917485674305,"d":"3.51"},{"$f":"VLOOKUP(A1862,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":2.6980271536084115,"d":"2.70"}]
["05027","05","AR","027","Columbia","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.149115350650054,"A","CEC Survey",2017,15,"I",14.572903609942648,"TON",8,{"v":3.512291748567431,"d":"3.51"},{"$f":"VLOOKUP(A1863,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":2.698027153608412,"d":"2.70"}]
["05027","05","AR","027","Columbia","","2104008610","Hydronic heater: outdoor","Hydronic heater",49.78938420780065,"A","CEC Survey",2017,15,"I",174.87484331931176,"TON",8,{"v":3.5122917485674305,"d":"3.51"},{"$f":"VLOOKUP(A1864,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":2.6980271536084115,"d":"2.70"}]
["05027","05","AR","027","Columbia","","2104008620","Hydronic heater: indoor","Hydronic heater",31.80988435498375,"A","CEC Survey",2017,15,"I",111.72559434289364,"TON",8,{"v":3.512291748567431,"d":"3.51"},{"$f":"VLOOKUP(A1865,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":2.698027153608412,"d":"2.70"}]
["05027","05","AR","027","Columbia","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.3830384502166848,"A","CEC Survey",2017,15,"I",4.8576345366475495,"TON",8,{"v":3.512291748567431,"d":"3.51"},{"$f":"VLOOKUP(A1866,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":2.698027153608412,"d":"2.70"}]
["05027","05","AR","027","Columbia","","2104008100","Fireplace: general","Fireplace: general",1643.137967657,"A","CEC Survey",2017,15,"I",924.8595501974249,"TON",8,{"v":0.5628617732668,"d":"0.56"},{"$f":"VLOOKUP(A1867,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":0.43237192599999996,"d":"0.43"}]
["05027","05","AR","027","Columbia","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",243.66414047315,"A","CEC Survey",2017,15,"I",381.4899367325296,"TON",8,{"v":1.5656384069964,"d":"1.57"},{"$f":"VLOOKUP(A1868,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":1.202671998,"d":"1.20"}]
["05027","05","AR","027","Columbia","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",322.26547610965,"A","CEC Survey",2017,15,"I",504.55120664624883,"TON",8,{"v":1.5656384069963998,"d":"1.57"},{"$f":"VLOOKUP(A1869,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":1.2026719979999998,"d":"1.20"}]
["05027","05","AR","027","Columbia","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",220.08373978220004,"A","CEC Survey",2017,15,"I",344.57155575841387,"TON",8,{"v":1.5656384069963998,"d":"1.57"},{"$f":"VLOOKUP(A1870,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":1.2026719979999998,"d":"1.20"}]
["05027","05","AR","027","Columbia","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1448.665232323,"A","CEC Survey",2017,15,"I",634.3799037164908,"TON",8,{"v":0.43790648768400003,"d":"0.44"},{"$f":"VLOOKUP(A1871,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":0.33638538,"d":"0.34"}]
["05027","05","AR","027","Columbia","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",323.249797122,"A","CEC Survey",2017,15,"I",191.58158055334076,"TON",8,{"v":0.592673475,"d":"0.59"},{"$f":"VLOOKUP(A1872,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":0.45527229605162084,"d":"0.46"}]
["05027","05","AR","027","Columbia","","2104009000","Wax Log; Total: All Combustor Types",null,134.10707121341417,"A","CEC Survey",2017,15,"I",31.39879702946045,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1873,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":0.17985274235673682,"d":"0.18"}]
["05027","05","AR","027","Columbia","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",305.76536192084,"A","CEC Survey",2017,15,"I",669.0719725494164,"TON",8,{"v":2.1881875970066003,"d":"2.19"},{"$f":"VLOOKUP(A1874,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":1.6808938370000002,"d":"1.68"}]
["05027","05","AR","027","Columbia","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",404.39934963724,"A","CEC Survey",2017,15,"I",884.9016411137442,"TON",8,{"v":2.1881875970066003,"d":"2.19"},{"$f":"VLOOKUP(A1875,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":1.6808938370000002,"d":"1.68"}]
["05027","05","AR","027","Columbia","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",276.17516560592003,"A","CEC Survey",2017,15,"I",604.323071980118,"TON",8,{"v":2.1881875970066003,"d":"2.19"},{"$f":"VLOOKUP(A1876,cordwood_density!A:D,4,FALSE)","v":1.3018},{"v":1.6808938370000002,"d":"1.68"}]
["05029","05","AR","029","Conway","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",49.183485762096616,"A","CEC Survey",2017,15,"I",168.59741479673255,"TON",8,{"v":3.4279273252865416,"d":"3.43"},{"$f":"VLOOKUP(A1877,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":2.7948857116074537,"d":"2.79"}]
["05029","05","AR","029","Conway","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.9878501969267526,"A","CEC Survey",2017,15,"I",13.670060659194531,"TON",8,{"v":3.4279273252865416,"d":"3.43"},{"$f":"VLOOKUP(A1878,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":2.7948857116074537,"d":"2.79"}]
["05029","05","AR","029","Conway","","2104008610","Hydronic heater: outdoor","Hydronic heater",47.85420236312103,"A","CEC Survey",2017,15,"I",164.04072791033437,"TON",8,{"v":3.427927325286541,"d":"3.43"},{"$f":"VLOOKUP(A1879,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":2.7948857116074532,"d":"2.79"}]
["05029","05","AR","029","Conway","","2104008620","Hydronic heater: indoor","Hydronic heater",30.57351817643844,"A","CEC Survey",2017,15,"I",104.80379838715808,"TON",8,{"v":3.4279273252865416,"d":"3.43"},{"$f":"VLOOKUP(A1880,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":2.7948857116074537,"d":"2.79"}]
["05029","05","AR","029","Conway","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.3292833989755843,"A","CEC Survey",2017,15,"I",4.556686886398177,"TON",8,{"v":3.427927325286541,"d":"3.43"},{"$f":"VLOOKUP(A1881,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":2.7948857116074532,"d":"2.79"}]
["05029","05","AR","029","Conway","","2104008100","Fireplace: general","Fireplace: general",826.3527216390406,"A","CEC Survey",2017,15,"I",479.90771863738075,"TON",8,{"v":0.5807540848725,"d":"0.58"},{"$f":"VLOOKUP(A1882,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":0.47350516500000006,"d":"0.47"}]
["05029","05","AR","029","Conway","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",206.8707595134256,"A","CEC Survey",2017,15,"I",214.68082463084804,"TON",8,{"v":1.0377533544895,"d":"1.04"},{"$f":"VLOOKUP(A1883,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":0.846109543,"d":"0.85"}]
["05029","05","AR","029","Conway","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",273.6032625822726,"A","CEC Survey",2017,15,"I",283.93270354402483,"TON",8,{"v":1.0377533544895,"d":"1.04"},{"$f":"VLOOKUP(A1884,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":0.846109543,"d":"0.85"}]
["05029","05","AR","029","Conway","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",186.85100859277154,"A","CEC Survey",2017,15,"I",193.90526095689503,"TON",8,{"v":1.0377533544895,"d":"1.04"},{"$f":"VLOOKUP(A1885,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":0.846109543,"d":"0.85"}]
["05029","05","AR","029","Conway","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1281.080881568484,"A","CEC Survey",2017,15,"I",523.798250917819,"TON",8,{"v":0.408872116081,"d":"0.41"},{"$f":"VLOOKUP(A1886,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":0.333364954,"d":"0.33"}]
["05029","05","AR","029","Conway","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",314.6192943465615,"A","CEC Survey",2017,15,"I",175.56492110062527,"TON",8,{"v":0.558023377,"d":"0.56"},{"$f":"VLOOKUP(A1887,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":0.4549721785568692,"d":"0.45"}]
["05029","05","AR","029","Conway","","2104009000","Wax Log; Total: All Combustor Types",null,117.5609272515463,"A","CEC Survey",2017,15,"I",40.373802294839486,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1888,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":0.2800071341214839,"d":"0.28"}]
["05029","05","AR","029","Conway","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",319.28177384579186,"A","CEC Survey",2017,15,"I",652.677469809476,"TON",8,{"v":2.0442052233295005,"d":"2.04"},{"$f":"VLOOKUP(A1889,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":1.6666981030000005,"d":"1.67"}]
["05029","05","AR","029","Conway","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",422.2758944412086,"A","CEC Survey",2017,15,"I",863.2185891028552,"TON",8,{"v":2.0442052233295,"d":"2.04"},{"$f":"VLOOKUP(A1890,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":1.666698103,"d":"1.67"}]
["05029","05","AR","029","Conway","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",288.3835376671669,"A","CEC Survey",2017,15,"I",589.5151340214621,"TON",8,{"v":2.0442052233295,"d":"2.04"},{"$f":"VLOOKUP(A1891,cordwood_density!A:D,4,FALSE)","v":1.2265},{"v":1.666698103,"d":"1.67"}]
["05031","05","AR","031","Craighead","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",121.9409033950292,"A","CEC Survey",2017,15,"I",448.09638405573315,"TON",8,{"v":3.674701200171684,"d":"3.67"},{"$f":"VLOOKUP(A1892,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":2.7266462863928798,"d":"2.73"}]
["05031","05","AR","031","Craighead","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",9.887100275272637,"A","CEC Survey",2017,15,"I",36.33213924776215,"TON",8,{"v":3.6747012001716843,"d":"3.67"},{"$f":"VLOOKUP(A1893,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":2.72664628639288,"d":"2.73"}]
["05031","05","AR","031","Craighead","","2104008610","Hydronic heater: outdoor","Hydronic heater",118.64520330327164,"A","CEC Survey",2017,15,"I",435.9856709731458,"TON",8,{"v":3.6747012001716843,"d":"3.67"},{"$f":"VLOOKUP(A1894,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":2.72664628639288,"d":"2.73"}]
["05031","05","AR","031","Craighead","","2104008620","Hydronic heater: indoor","Hydronic heater",75.80110211042356,"A","CEC Survey",2017,15,"I",278.5464008995098,"TON",8,{"v":3.674701200171684,"d":"3.67"},{"$f":"VLOOKUP(A1895,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":2.7266462863928798,"d":"2.73"}]
["05031","05","AR","031","Craighead","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.295700091757546,"A","CEC Survey",2017,15,"I",12.110713082587383,"TON",8,{"v":3.674701200171684,"d":"3.67"},{"$f":"VLOOKUP(A1896,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":2.7266462863928798,"d":"2.73"}]
["05031","05","AR","031","Craighead","","2104008100","Fireplace: general","Fireplace: general",2701.77073253,"A","CEC Survey",2017,15,"I",1636.5918954856713,"TON",8,{"v":0.6057478807437999,"d":"0.61"},{"$f":"VLOOKUP(A1897,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.449467894,"d":"0.45"}]
["05031","05","AR","031","Craighead","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",603.41526481068,"A","CEC Survey",2017,15,"I",445.2400180546801,"TON",8,{"v":0.7378666799129999,"d":"0.74"},{"$f":"VLOOKUP(A1898,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.54750069,"d":"0.55"}]
["05031","05","AR","031","Craighead","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",798.06535023348,"A","CEC Survey",2017,15,"I",588.8658303303833,"TON",8,{"v":0.7378666799129999,"d":"0.74"},{"$f":"VLOOKUP(A1899,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.54750069,"d":"0.55"}]
["05031","05","AR","031","Craighead","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",545.0202391838401,"A","CEC Survey",2017,15,"I",402.15227437196916,"TON",8,{"v":0.7378666799129998,"d":"0.74"},{"$f":"VLOOKUP(A1900,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.5475006899999999,"d":"0.55"}]
["05031","05","AR","031","Craighead","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4995.266502619999,"A","CEC Survey",2017,15,"I",2249.08344643837,"TON",8,{"v":0.4502429340374,"d":"0.45"},{"$f":"VLOOKUP(A1901,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.334082462,"d":"0.33"}]
["05031","05","AR","031","Craighead","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1150.302052134,"A","CEC Survey",2017,15,"I",375.8678201243027,"TON",8,{"v":0.326755759,"d":"0.33"},{"$f":"VLOOKUP(A1902,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.2424543733768643,"d":"0.24"}]
["05031","05","AR","031","Craighead","","2104009000","Wax Log; Total: All Combustor Types",null,572.1920855735241,"A","CEC Survey",2017,15,"I",196.50721270840842,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1903,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.2548258143503747,"d":"0.25"}]
["05031","05","AR","031","Craighead","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",951.9080874807801,"A","CEC Survey",2017,15,"I",1751.3908131672692,"TON",8,{"v":1.8398738661862997,"d":"1.84"},{"$f":"VLOOKUP(A1904,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":1.365195419,"d":"1.37"}]
["05031","05","AR","031","Craighead","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1258.9752124745798,"A","CEC Survey",2017,15,"I",2316.3555916083237,"TON",8,{"v":1.8398738661862999,"d":"1.84"},{"$f":"VLOOKUP(A1905,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":1.365195419,"d":"1.37"}]
["05031","05","AR","031","Craighead","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",859.7879499826402,"A","CEC Survey",2017,15,"I",1581.901379634953,"TON",8,{"v":1.8398738661862997,"d":"1.84"},{"$f":"VLOOKUP(A1906,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":1.365195419,"d":"1.37"}]
["05033","05","AR","033","Crawford","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",139.9868228749502,"A","CEC Survey",2017,15,"I",533.3063458677882,"TON",8,{"v":3.8096896187449665,"d":"3.81"},{"$f":"VLOOKUP(A1907,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":2.7777540056470773,"d":"2.78"}]
["05033","05","AR","033","Crawford","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.350282935806772,"A","CEC Survey",2017,15,"I",43.241055070361206,"TON",8,{"v":3.809689618744967,"d":"3.81"},{"$f":"VLOOKUP(A1908,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":2.7777540056470778,"d":"2.78"}]
["05033","05","AR","033","Crawford","","2104008610","Hydronic heater: outdoor","Hydronic heater",136.20339522968126,"A","CEC Survey",2017,15,"I",518.8926608443345,"TON",8,{"v":3.8096896187449674,"d":"3.81"},{"$f":"VLOOKUP(A1909,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":2.777754005647078,"d":"2.78"}]
["05033","05","AR","033","Crawford","","2104008620","Hydronic heater: indoor","Hydronic heater",87.01883584118526,"A","CEC Survey",2017,15,"I",331.51475553943595,"TON",8,{"v":3.809689618744967,"d":"3.81"},{"$f":"VLOOKUP(A1910,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":2.7777540056470778,"d":"2.78"}]
["05033","05","AR","033","Crawford","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.7834276452689246,"A","CEC Survey",2017,15,"I",14.413685023453736,"TON",8,{"v":3.8096896187449665,"d":"3.81"},{"$f":"VLOOKUP(A1911,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":2.7777540056470773,"d":"2.78"}]
["05033","05","AR","033","Crawford","","2104008100","Fireplace: general","Fireplace: general",3248.94512712,"A","CEC Survey",2017,15,"I",1940.3748405089873,"TON",8,{"v":0.597232259884,"d":"0.60"},{"$f":"VLOOKUP(A1912,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.435459176,"d":"0.44"}]
["05033","05","AR","033","Crawford","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",568.5423414516999,"A","CEC Survey",2017,15,"I",740.1022092162403,"TON",8,{"v":1.301753898094,"d":"1.30"},{"$f":"VLOOKUP(A1913,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.949146116,"d":"0.95"}]
["05033","05","AR","033","Crawford","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",751.9430967586999,"A","CEC Survey",2017,15,"I",978.8448573505113,"TON",8,{"v":1.301753898094,"d":"1.30"},{"$f":"VLOOKUP(A1914,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.949146116,"d":"0.95"}]
["05033","05","AR","033","Crawford","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",513.5221148596,"A","CEC Survey",2017,15,"I",668.4794147759591,"TON",8,{"v":1.3017538980939998,"d":"1.30"},{"$f":"VLOOKUP(A1915,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.9491461159999999,"d":"0.95"}]
["05033","05","AR","033","Crawford","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3760.11795467,"A","CEC Survey",2017,15,"I",1728.1125014839163,"TON",8,{"v":0.45958997093099996,"d":"0.46"},{"$f":"VLOOKUP(A1916,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.335100234,"d":"0.34"}]
["05033","05","AR","033","Crawford","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",867.3670544,"A","CEC Survey",2017,15,"I",514.7307080888163,"TON",8,{"v":0.593440465,"d":"0.59"},{"$f":"VLOOKUP(A1917,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.4326944695588772,"d":"0.43"}]
["05033","05","AR","033","Crawford","","2104009000","Wax Log; Total: All Combustor Types",null,342.84414585672016,"A","CEC Survey",2017,15,"I",117.74253645639108,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1918,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.25040375501275974,"d":"0.25"}]
["05033","05","AR","033","Crawford","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",828.650520698,"A","CEC Survey",2017,15,"I",1829.3482283916715,"TON",8,{"v":2.2076233378225,"d":"2.21"},{"$f":"VLOOKUP(A1919,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":1.609641515,"d":"1.61"}]
["05033","05","AR","033","Crawford","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1095.957140278,"A","CEC Survey",2017,15,"I",2419.46056013092,"TON",8,{"v":2.2076233378224996,"d":"2.21"},{"$f":"VLOOKUP(A1920,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":1.6096415149999999,"d":"1.61"}]
["05033","05","AR","033","Crawford","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",748.4585348240001,"A","CEC Survey",2017,15,"I",1652.314528869897,"TON",8,{"v":2.2076233378225,"d":"2.21"},{"$f":"VLOOKUP(A1921,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":1.609641515,"d":"1.61"}]
["05035","05","AR","035","Crittenden","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",40.168092474799565,"A","CEC Survey",2017,15,"I",128.73001010011131,"TON",8,{"v":3.2047827558869826,"d":"3.20"},{"$f":"VLOOKUP(A1922,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":2.630536613220867,"d":"2.63"}]
["05035","05","AR","035","Crittenden","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.2568723628215865,"A","CEC Survey",2017,15,"I",10.437568386495512,"TON",8,{"$f":"P1923/J1923","v":{"v":3.204782755886982,"d":"3.20"}},{"$f":"VLOOKUP(A1923,cordwood_density!A:D,4,FALSE)","v":1.2183},{"$f":"S1923/T1923","v":{"v":2.630536613220867,"d":"2.63"}}]
["05035","05","AR","035","Crittenden","","2104008610","Hydronic heater: outdoor","Hydronic heater",39.082468353859035,"A","CEC Survey",2017,15,"I",125.25082063794615,"TON",8,{"v":3.2047827558869826,"d":"3.20"},{"$f":"VLOOKUP(A1924,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":2.630536613220867,"d":"2.63"}]
["05035","05","AR","035","Crittenden","","2104008620","Hydronic heater: indoor","Hydronic heater",24.969354781632166,"A","CEC Survey",2017,15,"I",80.02135762979894,"TON",8,{"v":3.2047827558869826,"d":"3.20"},{"$f":"VLOOKUP(A1925,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":2.630536613220867,"d":"2.63"}]
["05035","05","AR","035","Crittenden","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0856241209405288,"A","CEC Survey",2017,15,"I",3.479189462165171,"TON",8,{"v":3.2047827558869826,"d":"3.20"},{"$f":"VLOOKUP(A1926,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":2.630536613220867,"d":"2.63"}]
["05035","05","AR","035","Crittenden","","2104008100","Fireplace: general","Fireplace: general",1398.521251335,"A","CEC Survey",2017,15,"I",771.7460722082612,"TON",8,{"v":0.5518300644138,"d":"0.55"},{"$f":"VLOOKUP(A1927,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":0.45295088600000005,"d":"0.45"}]
["05035","05","AR","035","Crittenden","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",261.19945402729,"A","CEC Survey",2017,15,"I",167.04576232903722,"TON",8,{"v":0.6395333518253998,"d":"0.64"},{"$f":"VLOOKUP(A1928,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":0.5249391379999999,"d":"0.52"}]
["05035","05","AR","035","Crittenden","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",345.45734242318997,"A","CEC Survey",2017,15,"I",220.9314921125976,"TON",8,{"v":0.6395333518253999,"d":"0.64"},{"$f":"VLOOKUP(A1929,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":0.524939138,"d":"0.52"}]
["05035","05","AR","035","Crittenden","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",235.92208750852,"A","CEC Survey",2017,15,"I",150.88004339396912,"TON",8,{"v":0.6395333518253999,"d":"0.64"},{"$f":"VLOOKUP(A1930,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":0.524939138,"d":"0.52"}]
["05035","05","AR","035","Crittenden","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2309.292230985,"A","CEC Survey",2017,15,"I",941.3472421182294,"TON",8,{"v":0.40763452519679994,"d":"0.41"},{"$f":"VLOOKUP(A1931,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":0.334592896,"d":"0.33"}]
["05035","05","AR","035","Crittenden","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",505.16072335900003,"A","CEC Survey",2017,15,"I",116.37181781542587,"TON",8,{"v":0.230365926,"d":"0.23"},{"$f":"VLOOKUP(A1932,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":0.1890880128047279,"d":"0.19"}]
["05035","05","AR","035","Crittenden","","2104009000","Wax Log; Total: All Combustor Types",null,190.88898135480002,"A","CEC Survey",2017,15,"I",65.55676425545228,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1933,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":0.28189177542477223,"d":"0.28"}]
["05035","05","AR","035","Crittenden","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",365.17531754826996,"A","CEC Survey",2017,15,"I",575.4435216372161,"TON",8,{"v":1.5758007017031,"d":"1.58"},{"$f":"VLOOKUP(A1934,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":1.293442257,"d":"1.29"}]
["05035","05","AR","035","Crittenden","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",482.9738070799699,"A","CEC Survey",2017,15,"I",761.0704641008342,"TON",8,{"v":1.5758007017031,"d":"1.58"},{"$f":"VLOOKUP(A1935,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":1.293442257,"d":"1.29"}]
["05035","05","AR","035","Crittenden","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",329.83577068876,"A","CEC Survey",2017,15,"I",519.7554388981308,"TON",8,{"v":1.5758007017031,"d":"1.58"},{"$f":"VLOOKUP(A1936,cordwood_density!A:D,4,FALSE)","v":1.2183},{"v":1.293442257,"d":"1.29"}]
["05037","05","AR","037","Cross","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",26.515476652900368,"A","CEC Survey",2017,15,"I",108.02831402797817,"TON",8,{"v":4.074160741747843,"d":"4.07"},{"$f":"VLOOKUP(A1937,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":2.76045852818473,"d":"2.76"}]
["05037","05","AR","037","Cross","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.149903512397327,"A","CEC Survey",2017,15,"I",8.759052488754987,"TON",8,{"v":4.074160741747844,"d":"4.07"},{"$f":"VLOOKUP(A1938,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":2.7604585281847305,"d":"2.76"}]
["05037","05","AR","037","Cross","","2104008610","Hydronic heater: outdoor","Hydronic heater",25.798842148767925,"A","CEC Survey",2017,15,"I",105.10862986505984,"TON",8,{"v":4.074160741747843,"d":"4.07"},{"$f":"VLOOKUP(A1939,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":2.76045852818473,"d":"2.76"}]
["05037","05","AR","037","Cross","","2104008620","Hydronic heater: indoor","Hydronic heater",16.482593595046175,"A","CEC Survey",2017,15,"I",67.15273574712157,"TON",8,{"v":4.074160741747843,"d":"4.07"},{"$f":"VLOOKUP(A1940,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":2.76045852818473,"d":"2.76"}]
["05037","05","AR","037","Cross","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7166345041324423,"A","CEC Survey",2017,15,"I",2.919684162918329,"TON",8,{"v":4.074160741747844,"d":"4.07"},{"$f":"VLOOKUP(A1941,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":2.7604585281847305,"d":"2.76"}]
["05037","05","AR","037","Cross","","2104008100","Fireplace: general","Fireplace: general",395.903397366,"A","CEC Survey",2017,15,"I",295.1610149504526,"TON",8,{"v":0.7455379693991,"d":"0.75"},{"$f":"VLOOKUP(A1942,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":0.505141249,"d":"0.51"}]
["05037","05","AR","037","Cross","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",133.0151308134,"A","CEC Survey",2017,15,"I",106.76820828077975,"TON",8,{"v":0.8026771663335002,"d":"0.80"},{"$f":"VLOOKUP(A1943,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":0.5438560650000002,"d":"0.54"}]
["05037","05","AR","037","Cross","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",175.9232375274,"A","CEC Survey",2017,15,"I",141.2095657907087,"TON",8,{"v":0.8026771663335001,"d":"0.80"},{"$f":"VLOOKUP(A1944,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":0.543856065,"d":"0.54"}]
["05037","05","AR","037","Cross","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",120.14269879920002,"A","CEC Survey",2017,15,"I",96.43580102780108,"TON",8,{"v":0.8026771663335001,"d":"0.80"},{"$f":"VLOOKUP(A1945,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":0.543856065,"d":"0.54"}]
["05037","05","AR","037","Cross","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,950.085649872,"A","CEC Survey",2017,15,"I",466.869557579063,"TON",8,{"v":0.4913973362738,"d":"0.49"},{"$f":"VLOOKUP(A1946,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":0.332947582,"d":"0.33"}]
["05037","05","AR","037","Cross","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",236.734127442,"A","CEC Survey",2017,15,"I",80.54421765674674,"TON",8,{"v":0.340230699,"d":"0.34"},{"$f":"VLOOKUP(A1947,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":0.23052422183074736,"d":"0.23"}]
["05037","05","AR","037","Cross","","2104009000","Wax Log; Total: All Combustor Types",null,96.60535086017177,"A","CEC Survey",2017,15,"I",33.177054889220216,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A1948,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":0.23269106985568128,"d":"0.23"}]
["05037","05","AR","037","Cross","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",216.62845339793998,"A","CEC Survey",2017,15,"I",479.8545222835392,"TON",8,{"v":2.2151038552727,"d":"2.22"},{"$f":"VLOOKUP(A1949,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":1.500849553,"d":"1.50"}]
["05037","05","AR","037","Cross","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",286.50859965534,"A","CEC Survey",2017,15,"I",634.646303665326,"TON",8,{"v":2.2151038552726994,"d":"2.22"},{"$f":"VLOOKUP(A1950,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":1.5008495529999997,"d":"1.50"}]
["05037","05","AR","037","Cross","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",195.66440952072,"A","CEC Survey",2017,15,"I",433.4169878690032,"TON",8,{"v":2.2151038552727,"d":"2.22"},{"$f":"VLOOKUP(A1951,cordwood_density!A:D,4,FALSE)","v":1.4759},{"v":1.500849553,"d":"1.50"}]
["05039","05","AR","039","Dallas","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",16.711114777471956,"A","CEC Survey",2017,15,"I",59.28180099611377,"TON",8,{"v":3.5474474196078662,"d":"3.55"},{"$f":"VLOOKUP(A1952,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":2.7410349402007927,"d":"2.74"}]
["05039","05","AR","039","Dallas","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.354955252227456,"A","CEC Survey",2017,15,"I",4.806632513198414,"TON",8,{"v":3.5474474196078662,"d":"3.55"},{"$f":"VLOOKUP(A1953,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":2.7410349402007927,"d":"2.74"}]
["05039","05","AR","039","Dallas","","2104008610","Hydronic heater: outdoor","Hydronic heater",16.25946302672947,"A","CEC Survey",2017,15,"I",57.67959015838097,"TON",8,{"v":3.5474474196078662,"d":"3.55"},{"$f":"VLOOKUP(A1954,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":2.7410349402007927,"d":"2.74"}]
["05039","05","AR","039","Dallas","","2104008620","Hydronic heater: indoor","Hydronic heater",10.387990267077162,"A","CEC Survey",2017,15,"I",36.85084926785451,"TON",8,{"v":3.547447419607866,"d":"3.55"},{"$f":"VLOOKUP(A1955,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":2.7410349402007927,"d":"2.74"}]
["05039","05","AR","039","Dallas","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.4516517507424853,"A","CEC Survey",2017,15,"I",1.6022108377328048,"TON",8,{"v":3.5474474196078662,"d":"3.55"},{"$f":"VLOOKUP(A1956,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":2.7410349402007927,"d":"2.74"}]
["05039","05","AR","039","Dallas","","2104008100","Fireplace: general","Fireplace: general",518.642930016,"A","CEC Survey",2017,15,"I",293.91624285239163,"TON",8,{"v":0.5667024957678,"d":"0.57"},{"$f":"VLOOKUP(A1957,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":0.437878609,"d":"0.44"}]
["05039","05","AR","039","Dallas","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",87.50282638031999,"A","CEC Survey",2017,15,"I",133.13217971826688,"TON",8,{"v":1.5214614798798003,"d":"1.52"},{"$f":"VLOOKUP(A1958,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":1.1755999690000003,"d":"1.18"}]
["05039","05","AR","039","Dallas","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",115.72954456751998,"A","CEC Survey",2017,15,"I",176.07804414351423,"TON",8,{"v":1.5214614798798,"d":"1.52"},{"$f":"VLOOKUP(A1959,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":1.175599969,"d":"1.18"}]
["05039","05","AR","039","Dallas","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",79.03481092416,"A","CEC Survey",2017,15,"I",120.24842039069267,"TON",8,{"v":1.5214614798798003,"d":"1.52"},{"$f":"VLOOKUP(A1960,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":1.1755999690000003,"d":"1.18"}]
["05039","05","AR","039","Dallas","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,484.913098224,"A","CEC Survey",2017,15,"I",210.73038838417452,"TON",8,{"v":0.4345735125654,"d":"0.43"},{"$f":"VLOOKUP(A1961,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":0.335785437,"d":"0.34"}]
["05039","05","AR","039","Dallas","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",105.564167016,"A","CEC Survey",2017,15,"I",63.15448423727522,"TON",8,{"v":0.598256833,"d":"0.60"},{"$f":"VLOOKUP(A1962,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":0.46225995441199197,"d":"0.46"}]
["05039","05","AR","039","Dallas","","2104009000","Wax Log; Total: All Combustor Types",null,45.157184523398755,"A","CEC Survey",2017,15,"I",10.572755473987753,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A1963,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":0.1809089012517385,"d":"0.18"}]
["05039","05","AR","039","Dallas","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",106.3623462432,"A","CEC Survey",2017,15,"I",232.59723321405065,"TON",8,{"v":2.1868381192176,"d":"2.19"},{"$f":"VLOOKUP(A1964,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":1.689721928,"d":"1.69"}]
["05039","05","AR","039","Dallas","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",140.67278051519997,"A","CEC Survey",2017,15,"I",307.6285987669702,"TON",8,{"v":2.1868381192176,"d":"2.19"},{"$f":"VLOOKUP(A1965,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":1.689721928,"d":"1.69"}]
["05039","05","AR","039","Dallas","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",96.06921596160001,"A","CEC Survey",2017,15,"I",210.0878235481748,"TON",8,{"v":2.1868381192176,"d":"2.19"},{"$f":"VLOOKUP(A1966,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":1.689721928,"d":"1.69"}]
["05041","05","AR","041","Desha","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",13.993644425110379,"A","CEC Survey",2017,15,"I",45.48033675505856,"TON",8,{"v":3.250070916011561,"d":"3.25"},{"$f":"VLOOKUP(A1967,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":2.6348365756072645,"d":"2.63"}]
["05041","05","AR","041","Desha","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.1346198182521927,"A","CEC Survey",2017,15,"I",3.6875948720317746,"TON",8,{"v":3.250070916011561,"d":"3.25"},{"$f":"VLOOKUP(A1968,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":2.6348365756072645,"d":"2.63"}]
["05041","05","AR","041","Desha","","2104008610","Hydronic heater: outdoor","Hydronic heater",13.615437819026313,"A","CEC Survey",2017,15,"I",44.2511384643813,"TON",8,{"v":3.250070916011561,"d":"3.25"},{"$f":"VLOOKUP(A1969,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":2.6348365756072645,"d":"2.63"}]
["05041","05","AR","041","Desha","","2104008620","Hydronic heater: indoor","Hydronic heater",8.698751939933478,"A","CEC Survey",2017,15,"I",28.27156068557694,"TON",8,{"v":3.250070916011561,"d":"3.25"},{"$f":"VLOOKUP(A1970,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":2.6348365756072645,"d":"2.63"}]
["05041","05","AR","041","Desha","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.3782066060840643,"A","CEC Survey",2017,15,"I",1.2291982906772583,"TON",8,{"v":3.2500709160115604,"d":"3.25"},{"$f":"VLOOKUP(A1971,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":2.634836575607264,"d":"2.63"}]
["05041","05","AR","041","Desha","","2104008100","Fireplace: general","Fireplace: general",442.8312128,"A","CEC Survey",2017,15,"I",254.10685729199633,"TON",8,{"v":0.5738232761085,"d":"0.57"},{"$f":"VLOOKUP(A1972,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":0.46519925100000004,"d":"0.47"}]
["05041","05","AR","041","Desha","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",95.0100590867,"A","CEC Survey",2017,15,"I",75.12971054628197,"TON",8,{"v":0.7907553291565,"d":"0.79"},{"$f":"VLOOKUP(A1973,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":0.641066339,"d":"0.64"}]
["05041","05","AR","041","Desha","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",125.6584652437,"A","CEC Survey",2017,15,"I",99.36510104508261,"TON",8,{"v":0.7907553291565,"d":"0.79"},{"$f":"VLOOKUP(A1974,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":0.641066339,"d":"0.64"}]
["05041","05","AR","041","Desha","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",85.8155372396,"A","CEC Survey",2017,15,"I",67.8590933966418,"TON",8,{"v":0.7907553291565002,"d":"0.79"},{"$f":"VLOOKUP(A1975,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":0.6410663390000001,"d":"0.64"}]
["05041","05","AR","041","Desha","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,698.2964727,"A","CEC Survey",2017,15,"I",286.69526148159116,"TON",8,{"v":0.41056381163300004,"d":"0.41"},{"$f":"VLOOKUP(A1976,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":0.33284459800000005,"d":"0.33"}]
["05041","05","AR","041","Desha","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",153.17847321,"A","CEC Survey",2017,15,"I",43.28472292132751,"TON",8,{"v":0.282577062,"d":"0.28"},{"$f":"VLOOKUP(A1977,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":0.2290855792460478,"d":"0.23"}]
["05041","05","AR","041","Desha","","2104009000","Wax Log; Total: All Combustor Types",null,75.11834448389806,"A","CEC Survey",2017,15,"I",17.587630766207365,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1978,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":0.1898113498175922,"d":"0.19"}]
["05041","05","AR","041","Desha","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",124.6743366667,"A","CEC Survey",2017,15,"I",216.34675596042848,"TON",8,{"v":1.735295023376,"d":"1.74"},{"$f":"VLOOKUP(A1979,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":1.406805856,"d":"1.41"}]
["05041","05","AR","041","Desha","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",164.89186462369997,"A","CEC Survey",2017,15,"I",286.1360320766957,"TON",8,{"v":1.735295023376,"d":"1.74"},{"$f":"VLOOKUP(A1980,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":1.406805856,"d":"1.41"}]
["05041","05","AR","041","Desha","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",112.60907827960001,"A","CEC Survey",2017,15,"I",195.40997312554833,"TON",8,{"v":1.735295023376,"d":"1.74"},{"$f":"VLOOKUP(A1981,cordwood_density!A:D,4,FALSE)","v":1.2335},{"v":1.406805856,"d":"1.41"}]
["05043","05","AR","043","Drew","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",26.912936131272478,"A","CEC Survey",2017,15,"I",100.35936456994622,"TON",8,{"v":3.729038113137346,"d":"3.73"},{"$f":"VLOOKUP(A1982,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":2.8018920378220344,"d":"2.80"}]
["05043","05","AR","043","Drew","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.18212995658966,"A","CEC Survey",2017,15,"I",8.137245775941585,"TON",8,{"v":3.729038113137346,"d":"3.73"},{"$f":"VLOOKUP(A1983,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":2.8018920378220344,"d":"2.80"}]
["05043","05","AR","043","Drew","","2104008610","Hydronic heater: outdoor","Hydronic heater",26.185559479075923,"A","CEC Survey",2017,15,"I",97.64694931129902,"TON",8,{"v":3.729038113137346,"d":"3.73"},{"$f":"VLOOKUP(A1984,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":2.8018920378220344,"d":"2.80"}]
["05043","05","AR","043","Drew","","2104008620","Hydronic heater: indoor","Hydronic heater",16.72966300052073,"A","CEC Survey",2017,15,"I",62.38555094888549,"TON",8,{"v":3.7290381131373453,"d":"3.73"},{"$f":"VLOOKUP(A1985,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":2.8018920378220344,"d":"2.80"}]
["05043","05","AR","043","Drew","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7273766521965535,"A","CEC Survey",2017,15,"I",2.7124152586471952,"TON",8,{"v":3.729038113137346,"d":"3.73"},{"$f":"VLOOKUP(A1986,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":2.8018920378220344,"d":"2.80"}]
["05043","05","AR","043","Drew","","2104008100","Fireplace: general","Fireplace: general",747.747650844,"A","CEC Survey",2017,15,"I",431.500916990855,"TON",8,{"$f":"P1987/J1987","v":{"v":0.5770675661820001,"d":"0.58"}},{"$f":"VLOOKUP(A1987,cordwood_density!A:D,4,FALSE)","v":1.3309},{"$f":"S1987/T1987","v":{"v":0.43359198000000004,"d":"0.43"}}]
["05043","05","AR","043","Drew","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",171.26994381443998,"A","CEC Survey",2017,15,"I",208.04185981899292,"TON",8,{"v":1.2147015126273,"d":"1.21"},{"$f":"VLOOKUP(A1988,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":0.912691797,"d":"0.91"}]
["05043","05","AR","043","Drew","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",226.51831278683997,"A","CEC Survey",2017,15,"I",275.15213717995834,"TON",8,{"v":1.2147015126272998,"d":"1.21"},{"$f":"VLOOKUP(A1989,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":0.9126917969999998,"d":"0.91"}]
["05043","05","AR","043","Drew","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",154.69543312272,"A","CEC Survey",2017,15,"I",187.9087766107033,"TON",8,{"v":1.2147015126273,"d":"1.21"},{"$f":"VLOOKUP(A1990,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":0.912691797,"d":"0.91"}]
["05043","05","AR","043","Drew","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,906.84073998,"A","CEC Survey",2017,15,"I",404.41240714941097,"TON",8,{"v":0.4459574755743,"d":"0.45"},{"$f":"VLOOKUP(A1991,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":0.335079627,"d":"0.34"}]
["05043","05","AR","043","Drew","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",194.878757304,"A","CEC Survey",2017,15,"I",99.10632905840933,"TON",8,{"v":0.508553782,"d":"0.51"},{"$f":"VLOOKUP(A1992,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":0.3821126921631979,"d":"0.38"}]
["05043","05","AR","043","Drew","","2104009000","Wax Log; Total: All Combustor Types",null,101.08659817928766,"A","CEC Survey",2017,15,"I",23.66763773089243,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A1993,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":0.17592027951010594,"d":"0.18"}]
["05043","05","AR","043","Drew","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",210.45053232396,"A","CEC Survey",2017,15,"I",457.876453173782,"TON",8,{"v":2.1756963411665,"d":"2.18"},{"$f":"VLOOKUP(A1994,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":1.6347556849999998,"d":"1.63"}]
["05043","05","AR","043","Drew","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",278.33780081556,"A","CEC Survey",2017,15,"I",605.5785348427439,"TON",8,{"v":2.1756963411665,"d":"2.18"},{"$f":"VLOOKUP(A1995,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":1.6347556849999998,"d":"1.63"}]
["05043","05","AR","043","Drew","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",190.08435177648002,"A","CEC Survey",2017,15,"I",413.56582867309345,"TON",8,{"v":2.1756963411665,"d":"2.18"},{"$f":"VLOOKUP(A1996,cordwood_density!A:D,4,FALSE)","v":1.3309},{"v":1.6347556849999998,"d":"1.63"}]
["05045","05","AR","045","Faulkner","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",155.90558757665204,"A","CEC Survey",2017,15,"I",586.66940044492,"TON",8,{"v":3.762978669103056,"d":"3.76"},{"$f":"VLOOKUP(A1997,cordwood_density!A:D,4,FALSE)","v":1.3911},{"v":2.705038220906517,"d":"2.71"}]
["05045","05","AR","045","Faulkner","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",12.64099358729611,"A","CEC Survey",2017,15,"I",47.56778922526379,"TON",8,{"v":3.7629786691030565,"d":"3.76"},{"$f":"VLOOKUP(A1998,cordwood_density!A:D,4,FALSE)","v":1.3911},{"v":2.7050382209065176,"d":"2.71"}]
["05045","05","AR","045","Faulkner","","2104008610","Hydronic heater: outdoor","Hydronic heater",151.69192304755333,"A","CEC Survey",2017,15,"I",570.8134707031654,"TON",8,{"v":3.762978669103056,"d":"3.76"},{"$f":"VLOOKUP(A1999,cordwood_density!A:D,4,FALSE)","v":1.3911},{"v":2.705038220906517,"d":"2.71"}]
["05045","05","AR","045","Faulkner","","2104008620","Hydronic heater: indoor","Hydronic heater",96.91428416927019,"A","CEC Survey",2017,15,"I",364.68638406035575,"TON",8,{"v":3.7629786691030565,"d":"3.76"},{"$f":"VLOOKUP(A2000,cordwood_density!A:D,4,FALSE)","v":1.3911},{"v":2.7050382209065176,"d":"2.71"}]
["05045","05","AR","045","Faulkner","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1108.6449701184,"A","CEC Survey",2017,15,"I",1176.836118679535,"TON",8,{"v":1.0615085535939,"d":"1.06"},{"$f":"VLOOKUP(A2004,cordwood_density!A:D,4,FALSE)","v":1.3911},{"v":0.763071349,"d":"0.76"}]
["05047","05","AR","047","Franklin","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",366.98803035687996,"A","CEC Survey",2017,15,"I",895.3974608934135,"TON",8,{"v":2.4398546732510002,"d":"2.44"},{"$f":"VLOOKUP(A2025,cordwood_density!A:D,4,FALSE)","v":1.4207},{"v":1.7173609300000001,"d":"1.72"}]
["05053","05","AR","053","Grant","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",242.07311095603998,"A","CEC Survey",2017,15,"I",340.58094272211054,"TON",8,{"v":1.4069342165968999,"d":"1.41"},{"$f":"VLOOKUP(A2064,cordwood_density!A:D,4,FALSE)","v":1.2821},{"v":1.097366989,"d":"1.10"}]
["05055","05","AR","055","Greene","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",556.338510945,"A","CEC Survey",2017,15,"I",238.44055104626682,"TON",8,{"v":0.428588973,"d":"0.43"},{"$f":"VLOOKUP(A2082,cordwood_density!A:D,4,FALSE)","v":1.3477},{"v":0.31801511686577133,"d":"0.32"}]
["05059","05","AR","059","Hot Spring","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.2924967334574085,"A","CEC Survey",2017,15,"I",23.563387296700174,"TON",8,{"v":3.7446800999375784,"d":"3.74"},{"$f":"VLOOKUP(A2103,cordwood_density!A:D,4,FALSE)","v":1.3161},{"v":2.84528538860085,"d":"2.85"}]
["05061","05","AR","061","Howard","","2104008620","Hydronic heater: indoor","Hydronic heater",17.787692430767812,"A","CEC Survey",2017,15,"I",62.58636654132719,"TON",8,{"v":3.5185208415831384,"d":"3.52"},{"$f":"VLOOKUP(A2120,cordwood_density!A:D,4,FALSE)","v":1.3121},{"v":2.681595032073118,"d":"2.68"}]
["05063","05","AR","063","Independence","","2104008620","Hydronic heater: indoor","Hydronic heater",57.172984749693065,"A","CEC Survey",2017,15,"I",232.5186565105989,"TON",8,{"v":4.066932267548743,"d":"4.07"},{"$f":"VLOOKUP(A2135,cordwood_density!A:D,4,FALSE)","v":1.4162},{"v":2.8717216971817137,"d":"2.87"}]
["05065","05","AR","065","Izard","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",298.73080492916,"A","CEC Survey",2017,15,"I",771.1727056017957,"TON",8,{"v":2.5814970966408,"d":"2.58"},{"$f":"VLOOKUP(A2159,cordwood_density!A:D,4,FALSE)","v":1.4092},{"v":1.831888374,"d":"1.83"}]
["05069","05","AR","069","Jefferson","","2104008620","Hydronic heater: indoor","Hydronic heater",48.112240825753176,"A","CEC Survey",2017,15,"I",175.95153728532267,"TON",8,{"v":3.657105432327745,"d":"3.66"},{"$f":"VLOOKUP(A2180,cordwood_density!A:D,4,FALSE)","v":1.3976},{"v":2.616703944138341,"d":"2.62"}]
["05073","05","AR","073","Lafayette","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.4995023030976445,"A","CEC Survey",2017,15,"I",1.7661360073886738,"TON",8,{"v":3.5357915197508576,"d":"3.54"},{"$f":"VLOOKUP(A2211,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":2.7651454756790943,"d":"2.77"}]
["05077","05","AR","077","Lee","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",13.875002228372434,"A","CEC Survey",2017,15,"I",55.61640748880402,"TON",8,{"v":4.008389085161822,"d":"4.01"},{"$f":"VLOOKUP(A2237,cordwood_density!A:D,4,FALSE)","v":1.5085},{"v":2.65720191260313,"d":"2.66"}]
["05079","05","AR","079","Lincoln","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",96.69278578448,"A","CEC Survey",2017,15,"I",91.75390764905457,"TON",8,{"v":0.9489219583926999,"d":"0.95"},{"$f":"VLOOKUP(A2258,cordwood_density!A:D,4,FALSE)","v":1.4279},{"v":0.664557713,"d":"0.66"}]
["05083","05","AR","083","Logan","","2104008100","Fireplace: general","Fireplace: general",1034.009053705,"A","CEC Survey",2017,15,"I",671.1172853229397,"TON",8,{"v":0.6490439159292,"d":"0.65"},{"$f":"VLOOKUP(A2287,cordwood_density!A:D,4,FALSE)","v":1.3673},{"v":0.474690204,"d":"0.47"}]
["05083","05","AR","083","Logan","","2104009000","Wax Log; Total: All Combustor Types",null,118.76741692874819,"A","CEC Survey",2017,15,"I",40.788145536568834,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A2293,cordwood_density!A:D,4,FALSE)","v":1.3673},{"v":0.25117293205587654,"d":"0.25"}]
["05087","05","AR","087","Madison","","2104008610","Hydronic heater: outdoor","Hydronic heater",65.97227501457495,"A","CEC Survey",2017,15,"I",285.37225983253967,"TON",8,{"v":4.325639213889375,"d":"4.33"},{"$f":"VLOOKUP(A2314,cordwood_density!A:D,4,FALSE)","v":1.4098},{"v":3.068264444523603,"d":"3.07"}]
["05089","05","AR","089","Marion","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",478.49314274766,"A","CEC Survey",2017,15,"I",1259.030767820321,"TON",8,{"v":2.6312409841247995,"d":"2.63"},{"$f":"VLOOKUP(A2340,cordwood_density!A:D,4,FALSE)","v":1.4472},{"v":1.8181598839999995,"d":"1.82"}]
["05095","05","AR","095","Monroe","","2104008620","Hydronic heater: indoor","Hydronic heater",10.03769827163207,"A","CEC Survey",2017,15,"I",35.62476305431367,"TON",8,{"v":3.549096823820078,"d":"3.55"},{"$f":"VLOOKUP(A2375,cordwood_density!A:D,4,FALSE)","v":1.3521},{"v":2.624877467509857,"d":"2.62"}]
["05097","05","AR","097","Montgomery","","2104008100","Fireplace: general","Fireplace: general",448.45470972,"A","CEC Survey",2017,15,"I",303.3821701202673,"TON",8,{"v":0.67650570625,"d":"0.68"},{"$f":"VLOOKUP(A2392,cordwood_density!A:D,4,FALSE)","v":1.375},{"v":0.49200415,"d":"0.49"}]
["05099","05","AR","099","Nevada","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",125.77705971088,"A","CEC Survey",2017,15,"I",179.23840015517646,"TON",8,{"v":1.4250484195383997,"d":"1.43"},{"$f":"VLOOKUP(A2409,cordwood_density!A:D,4,FALSE)","v":1.3256},{"v":1.075021439,"d":"1.08"}]
["05101","05","AR","101","Newton","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,576.57882776,"A","CEC Survey",2017,15,"I",277.790778992623,"TON",8,{"v":0.4817915012104,"d":"0.48"},{"$f":"VLOOKUP(A2426,cordwood_density!A:D,4,FALSE)","v":1.4299},{"v":0.336940696,"d":"0.34"}]
["05105","05","AR","105","Perry","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.7159705326988957,"A","CEC Survey",2017,15,"I",10.522428124587753,"TON",8,{"v":3.87427919335026,"d":"3.87"},{"$f":"VLOOKUP(A2448,cordwood_density!A:D,4,FALSE)","v":1.3112},{"v":2.9547583841902534,"d":"2.95"}]
["05107","05","AR","107","Phillips","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",147.7663642486,"A","CEC Survey",2017,15,"I",116.0677009598071,"TON",8,{"v":0.7854811989860998,"d":"0.79"},{"$f":"VLOOKUP(A2469,cordwood_density!A:D,4,FALSE)","v":1.3217},{"v":0.5942961329999998,"d":"0.59"}]
["05111","05","AR","111","Poinsett","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",365.487498771,"A","CEC Survey",2017,15,"I",129.7041688425401,"TON",8,{"v":0.354879905,"d":"0.35"},{"$f":"VLOOKUP(A2502,cordwood_density!A:D,4,FALSE)","v":1.3714},{"v":0.25877198847892663,"d":"0.26"}]
["05115","05","AR","115","Pope","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.7295666987969187,"A","CEC Survey",2017,15,"I",14.367140676888184,"TON",8,{"v":3.852227842318178,"d":"3.85"},{"$f":"VLOOKUP(A2526,cordwood_density!A:D,4,FALSE)","v":1.3583},{"v":2.836065554235572,"d":"2.84"}]
["05117","05","AR","117","Prairie","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",160.11944032,"A","CEC Survey",2017,15,"I",71.92140446287287,"TON",8,{"v":0.44917346900000005,"d":"0.45"},{"$f":"VLOOKUP(A2547,cordwood_density!A:D,4,FALSE)","v":1.2398},{"v":0.3622951032424585,"d":"0.36"}]
["05121","05","AR","121","Randolph","","2104009000","Wax Log; Total: All Combustor Types",null,105.40985281882337,"A","CEC Survey",2017,15,"I",36.20077399125248,"TON",8,{"v":0.34342874999999995,"d":"0.34"},{"$f":"VLOOKUP(A2578,cordwood_density!A:D,4,FALSE)","v":1.3929},{"v":0.24655664441094116,"d":"0.25"}]
["05123","05","AR","123","St Francis","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",33.95047383068965,"A","CEC Survey",2017,15,"I",129.35654427551682,"TON",8,{"v":3.8101543124439257,"d":"3.81"},{"$f":"VLOOKUP(A2582,cordwood_density!A:D,4,FALSE)","v":1.4136},{"v":2.6953553427022676,"d":"2.70"}]
["05125","05","AR","125","Saline","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1078.09639548558,"A","CEC Survey",2017,15,"I",1488.8608093878101,"TON",8,{"v":1.3810089854879999,"d":"1.38"},{"$f":"VLOOKUP(A2603,cordwood_density!A:D,4,FALSE)","v":1.269},{"v":1.088265552,"d":"1.09"}]
["05129","05","AR","129","Searcy","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0263389025654517,"A","CEC Survey",2017,15,"I",4.631980169439658,"TON",8,{"v":4.513109809889787,"d":"4.51"},{"$f":"VLOOKUP(A2631,cordwood_density!A:D,4,FALSE)","v":1.4439},{"v":3.125638762995905,"d":"3.13"}]
["05133","05","AR","133","Sevier","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",225.73186306879998,"A","CEC Survey",2017,15,"I",284.1862881299935,"TON",8,{"v":1.2589551349397998,"d":"1.26"},{"$f":"VLOOKUP(A2664,cordwood_density!A:D,4,FALSE)","v":1.3578},{"v":0.9272021909999999,"d":"0.93"}]
["05135","05","AR","135","Sharp","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1216.8780103679999,"A","CEC Survey",2017,15,"I",592.0027653480425,"TON",8,{"v":0.4864931080224,"d":"0.49"},{"$f":"VLOOKUP(A2681,cordwood_density!A:D,4,FALSE)","v":1.4496},{"v":0.335605069,"d":"0.34"}]
["05139","05","AR","139","Union","","2104008100","Fireplace: general","Fireplace: general",3036.116207636,"A","CEC Survey",2017,15,"I",1700.1999221110661,"TON",8,{"v":0.559991715019,"d":"0.56"},{"$f":"VLOOKUP(A2707,cordwood_density!A:D,4,FALSE)","v":1.3049},{"v":0.42914531000000006,"d":"0.43"}]
["05141","05","AR","141","Van Buren","","2104008620","Hydronic heater: indoor","Hydronic heater",41.339286665297,"A","CEC Survey",2017,15,"I",180.73759395765885,"TON",8,{"v":4.372054008115777,"d":"4.37"},{"$f":"VLOOKUP(A2720,cordwood_density!A:D,4,FALSE)","v":1.4035},{"v":3.1151079502071797,"d":"3.12"}]
["05143","05","AR","143","Washington","","2104008100","Fireplace: general","Fireplace: general",10377.57266604,"A","CEC Survey",2017,15,"I",5567.4413897717695,"TON",8,{"v":0.5364878251338,"d":"0.54"},{"$f":"VLOOKUP(A2737,cordwood_density!A:D,4,FALSE)","v":1.4121},{"v":0.37992197800000005,"d":"0.38"}]
["05145","05","AR","145","White","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1301.01042847287,"A","CEC Survey",2017,15,"I",2817.1698150193474,"TON",8,{"v":2.1653706637279995,"d":"2.17"},{"$f":"VLOOKUP(A2760,cordwood_density!A:D,4,FALSE)","v":1.361},{"v":1.5910144479999997,"d":"1.59"}]
["06001","06","CA","001","Alameda","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",4394.9519149797,"A","CEC Survey",2017,15,"I",2639.1594898303133,"TON",8,{"v":0.6004979214528001,"d":"0.60"},{"$f":"VLOOKUP(A2798,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5843693280000001,"d":"0.58"}]
["06003","06","CA","003","Alpine","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",5.17436214848,"A","CEC Survey",2017,15,"I",3.77675636635106,"TON",8,{"v":0.7298979580431,"d":"0.73"},{"$f":"VLOOKUP(A2815,cordwood_density!A:D,4,FALSE)","v":1.0367},{"v":0.704058993,"d":"0.70"}]
["06005","06","CA","005","Amador","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",470.0866229388,"A","CEC Survey",2017,15,"I",812.1251993505454,"TON",8,{"v":1.7276075508668003,"d":"1.73"},{"$f":"VLOOKUP(A2836,cordwood_density!A:D,4,FALSE)","v":1.0394},{"v":1.662120022,"d":"1.66"}]
["06011","06","CA","011","Colusa","","2104008610","Hydronic heater: outdoor","Hydronic heater",24.317721585230757,"A","CEC Survey",2017,15,"I",75.13675289133728,"TON",8,{"v":3.089794108711698,"d":"3.09"},{"$f":"VLOOKUP(A2869,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.0068062560448596,"d":"3.01"}]
["06011","06","CA","011","Colusa","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.67549226625641,"A","CEC Survey",2017,15,"I",2.087132024759369,"TON",8,{"v":3.089794108711698,"d":"3.09"},{"$f":"VLOOKUP(A2871,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.0068062560448596,"d":"3.01"}]
["06017","06","CA","017","El Dorado","","2104008610","Hydronic heater: outdoor","Hydronic heater",332.70546936408317,"A","CEC Survey",2017,15,"I",1080.1736992762524,"TON",8,{"v":3.2466364359469146,"d":"3.25"},{"$f":"VLOOKUP(A2914,cordwood_density!A:D,4,FALSE)","v":1.0485},{"v":3.096458212634158,"d":"3.10"}]
["06017","06","CA","017","El Dorado","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2330.425857624,"A","CEC Survey",2017,15,"I",1317.5234454984284,"TON",8,{"v":0.565357375,"d":"0.57"},{"$f":"VLOOKUP(A2922,cordwood_density!A:D,4,FALSE)","v":1.0485},{"v":0.5392058893657606,"d":"0.54"}]
["06021","06","CA","021","Glenn","","2104009000","Wax Log; Total: All Combustor Types",null,330.2941300231433,"A","CEC Survey",2017,15,"I",53.30696402272249,"TON",8,{"v":0.16139240506329114,"d":"0.16"},{"$f":"VLOOKUP(A2953,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.15869459691572385,"d":"0.16"}]
["06023","06","CA","023","Humboldt","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1859.5330483499,"A","CEC Survey",2017,15,"I",3390.3834477930723,"TON",8,{"v":1.8232445241033002,"d":"1.82"},{"$f":"VLOOKUP(A2970,cordwood_density!A:D,4,FALSE)","v":1.0837},{"v":1.682425509,"d":"1.68"}]
["06027","06","CA","027","Inyo","","2104009000","Wax Log; Total: All Combustor Types",null,459.4802766393443,"A","CEC Survey",2017,15,"I",74.01024590163935,"TON",8,{"v":0.1610738255033557,"d":"0.16"},{"$f":"VLOOKUP(A2998,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.15838134267783255,"d":"0.16"}]
["06029","06","CA","029","Kern","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",4231.273123671991,"A","CEC Survey",2017,15,"I",2371.259937105211,"TON",8,{"v":0.5604128752263999,"d":"0.56"},{"$f":"VLOOKUP(A3009,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5453609139999999,"d":"0.55"}]
["06035","06","CA","035","Lassen","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",9.303797799322004,"A","CEC Survey",2017,15,"I",31.888867533787113,"TON",8,{"v":3.4275108102748058,"d":"3.43"},{"$f":"VLOOKUP(A3048,cordwood_density!A:D,4,FALSE)","v":0.9579},{"v":3.5781509659409183,"d":"3.58"}]
["06035","06","CA","035","Lassen","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.101265933107335,"A","CEC Survey",2017,15,"I",10.62962251126237,"TON",8,{"v":3.427510810274805,"d":"3.43"},{"$f":"VLOOKUP(A3051,cordwood_density!A:D,4,FALSE)","v":0.9579},{"v":3.5781509659409174,"d":"3.58"}]
["06039","06","CA","039","Madera","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1506.8029458820001,"A","CEC Survey",2017,15,"I",554.5598309807373,"TON",8,{"v":0.368037395,"d":"0.37"},{"$f":"VLOOKUP(A3087,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.35815238906189173,"d":"0.36"}]
["06041","06","CA","041","Marin","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1633.25780633792,"A","CEC Survey",2017,15,"I",2124.655355672289,"TON",8,{"v":1.300869554964,"d":"1.30"},{"$f":"VLOOKUP(A3104,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2659298899999998,"d":"1.27"}]
["06043","06","CA","043","Mariposa","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1165.9711592031567,"A","CEC Survey",2017,15,"I",433.5435933509861,"TON",8,{"v":0.3718304607528,"d":"0.37"},{"$f":"VLOOKUP(A3116,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.361843578,"d":"0.36"}]
["06047","06","CA","047","Merced","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1164.56931250933,"A","CEC Survey",2017,15,"I",676.8801935416285,"TON",8,{"v":0.5812279151363999,"d":"0.58"},{"$f":"VLOOKUP(A3143,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5656168889999998,"d":"0.57"}]
["06053","06","CA","053","Monterey","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",172.18993278910148,"A","CEC Survey",2017,15,"I",480.67286659284923,"TON",8,{"v":2.791527116637987,"d":"2.79"},{"$f":"VLOOKUP(A3182,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.716550327596328,"d":"2.72"}]
["06053","06","CA","053","Monterey","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2860.677559993,"A","CEC Survey",2017,15,"I",536.6193991015701,"TON",8,{"v":0.18758472,"d":"0.19"},{"$f":"VLOOKUP(A3192,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.18254643830284156,"d":"0.18"}]
["06057","06","CA","057","Nevada","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,6364.07757408,"A","CEC Survey",2017,15,"I",2498.0924427361642,"TON",8,{"v":0.39253016853699996,"d":"0.39"},{"$f":"VLOOKUP(A3221,cordwood_density!A:D,4,FALSE)","v":1.079},{"v":0.363790703,"d":"0.36"}]
["06061","06","CA","061","Placer","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",441.90847071220935,"A","CEC Survey",2017,15,"I",1326.3734246264175,"TON",8,{"v":3.001466395266751,"d":"3.00"},{"$f":"VLOOKUP(A3242,cordwood_density!A:D,4,FALSE)","v":1.0256},{"v":2.9265467972569725,"d":"2.93"}]
["06063","06","CA","063","Plumas","","2104008610","Hydronic heater: outdoor","Hydronic heater",66.1267911027256,"A","CEC Survey",2017,15,"I",211.1062372516989,"TON",8,{"v":3.1924464159126202,"d":"3.19"},{"$f":"VLOOKUP(A3259,cordwood_density!A:D,4,FALSE)","v":0.9737},{"v":3.278675583765657,"d":"3.28"}]
["06067","06","CA","067","Sacramento","","2104008610","Hydronic heater: outdoor","Hydronic heater",750.1208814373414,"A","CEC Survey",2017,15,"I",806.908825937864,"TON",8,{"v":1.075705057552469,"d":"1.08"},{"$f":"VLOOKUP(A3289,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.046813018248802,"d":"1.05"}]
["06067","06","CA","067","Sacramento","","2104009000","Wax Log; Total: All Combustor Types",null,20782.306373900326,"A","CEC Survey",2017,15,"I",3355.3104849341994,"TON",8,{"v":0.1614503426408919,"d":"0.16"},{"$f":"VLOOKUP(A3298,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.15711399634185663,"d":"0.16"}]
["06073","06","CA","073","San Diego","","2104008100","Fireplace: general","Fireplace: general",69729.92768284901,"A","CEC Survey",2017,15,"I",28284.552485854198,"TON",8,{"v":0.40563002753280003,"d":"0.41"},{"$f":"VLOOKUP(A3337,cordwood_density!A:D,4,FALSE)","v":1.0304},{"v":0.39366268200000004,"d":"0.39"}]
["06073","06","CA","073","San Diego","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",18882.989194988,"A","CEC Survey",2017,15,"I",3498.5296403796615,"TON",8,{"v":0.185274143,"d":"0.19"},{"$f":"VLOOKUP(A3342,cordwood_density!A:D,4,FALSE)","v":1.0304},{"v":0.17980798039596274,"d":"0.18"}]
["06077","06","CA","077","San Joaquin","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",3201.44467878144,"A","CEC Survey",2017,15,"I",4028.2625581870316,"TON",8,{"v":1.2582639909056001,"d":"1.26"},{"$f":"VLOOKUP(A3376,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.224468656,"d":"1.22"}]
["06081","06","CA","081","San Mateo","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",25.37326628971888,"A","CEC Survey",2017,15,"I",20.97797560399234,"TON",8,{"v":0.8267747385953425,"d":"0.83"},{"$f":"VLOOKUP(A3393,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8045686440203799,"d":"0.80"}]
["06083","06","CA","083","Santa Barbara","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",131.6375293736404,"A","CEC Survey",2017,15,"I",357.5849428918512,"TON",8,{"v":2.716436145477031,"d":"2.72"},{"$f":"VLOOKUP(A3407,cordwood_density!A:D,4,FALSE)","v":1.0671},{"v":2.5456247263396414,"d":"2.55"}]
["06085","06","CA","085","Santa Clara","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",10570.97366299673,"A","CEC Survey",2017,15,"I",4031.4865815214675,"TON",8,{"v":0.38137325,"d":"0.38"},{"$f":"VLOOKUP(A3432,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3711300603347606,"d":"0.37"}]
["06091","06","CA","091","Sierra","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.3216274514590833,"A","CEC Survey",2017,15,"I",1.073291047364824,"TON",8,{"v":3.337062935690879,"d":"3.34"},{"$f":"VLOOKUP(A3471,cordwood_density!A:D,4,FALSE)","v":1.0192},{"v":3.274198327797173,"d":"3.27"}]
["06093","06","CA","093","Siskiyou","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",12.439528069432882,"A","CEC Survey",2017,15,"I",44.443119151139214,"TON",8,{"v":3.572733539654722,"d":"3.57"},{"$f":"VLOOKUP(A3483,cordwood_density!A:D,4,FALSE)","v":1.0727},{"v":3.330598992872865,"d":"3.33"}]
["06095","06","CA","095","Solano","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3048.20789880192,"A","CEC Survey",2017,15,"I",3766.9035541899866,"TON",8,{"v":1.2357764559531998,"d":"1.24"},{"$f":"VLOOKUP(A3510,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2025851069999998,"d":"1.20"}]
["06099","06","CA","099","Stanislaus","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",321.2259201982576,"A","CEC Survey",2017,15,"I",889.6839495050594,"TON",8,{"v":2.7696518044246083,"d":"2.77"},{"$f":"VLOOKUP(A3527,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.6952625578285403,"d":"2.70"}]
["06103","06","CA","103","Tehama","","2104008610","Hydronic heater: outdoor","Hydronic heater",105.63001867428675,"A","CEC Survey",2017,15,"I",338.8984886502723,"TON",8,{"v":3.2083539594485515,"d":"3.21"},{"$f":"VLOOKUP(A3559,cordwood_density!A:D,4,FALSE)","v":1.0141},{"v":3.163745152794154,"d":"3.16"}]
["06103","06","CA","103","Tehama","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3169.277534592,"A","CEC Survey",2017,15,"I",1164.451342513087,"TON",8,{"v":0.3674185456475,"d":"0.37"},{"$f":"VLOOKUP(A3566,cordwood_density!A:D,4,FALSE)","v":1.0141},{"v":0.362309975,"d":"0.36"}]
["06107","06","CA","107","Tulare","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",302.3539502491593,"A","CEC Survey",2017,15,"I",858.9389632457613,"TON",8,{"$f":"P3587/J3587","v":{"v":2.840839230107428,"d":"2.84"}},{"$f":"VLOOKUP(A3587,cordwood_density!A:D,4,FALSE)","v":1.0359},{"$f":"S3587/T3587","v":{"v":2.7423875182039077,"d":"2.74"}}]
["06109","06","CA","109","Tuolumne","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",813.6576008540001,"A","CEC Survey",2017,15,"I",386.93972311273603,"TON",8,{"v":0.475555962,"d":"0.48"},{"$f":"VLOOKUP(A3612,cordwood_density!A:D,4,FALSE)","v":0.9933},{"v":0.4787636786469345,"d":"0.48"}]
["06113","06","CA","113","Yolo","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1080.3097841556998,"A","CEC Survey",2017,15,"I",1427.5050665889185,"TON",8,{"v":1.3213849282172,"d":"1.32"},{"$f":"VLOOKUP(A3644,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.285894247,"d":"1.29"}]
["08001","08","CO","001","Adams","","2104008620","Hydronic heater: indoor","Hydronic heater",378.959256417522,"A","CEC Survey",2017,15,"I",969.4600359899116,"TON",8,{"v":2.5582170631077017,"d":"2.56"},{"$f":"VLOOKUP(A3665,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.4895066787735516,"d":"2.49"}]
["08003","08","CO","003","Alamosa","","2104008100","Fireplace: general","Fireplace: general",333.47804909900003,"A","CEC Survey",2017,15,"I",118.70447674234903,"TON",8,{"v":0.3559588916364,"d":"0.36"},{"$f":"VLOOKUP(A3682,cordwood_density!A:D,4,FALSE)","v":1.0188},{"v":0.349390353,"d":"0.35"}]
["08005","08","CO","005","Arapahoe","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1841.0499948161998,"A","CEC Survey",2017,15,"I",705.798704805001,"TON",8,{"v":0.3833674842032,"d":"0.38"},{"$f":"VLOOKUP(A3698,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.37307073199999996,"d":"0.37"}]
["08007","08","CO","007","Archuleta","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",227.99976761772,"A","CEC Survey",2017,15,"I",343.4928963082375,"TON",8,{"v":1.5065493263316003,"d":"1.51"},{"$f":"VLOOKUP(A3721,cordwood_density!A:D,4,FALSE)","v":1.0182},{"v":1.4796202380000003,"d":"1.48"}]
["08013","08","CO","013","Boulder","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1136.3356086544002,"A","CEC Survey",2017,15,"I",575.986838434419,"TON",8,{"v":0.506880919728,"d":"0.51"},{"$f":"VLOOKUP(A3760,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.498407984,"d":"0.50"}]
["08014","08","CO","014","Broomfield","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",290.53516231674,"A","CEC Survey",2017,15,"I",112.80911821420645,"TON",8,{"v":0.3882804315824,"d":"0.39"},{"$f":"VLOOKUP(A3774,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.377851724,"d":"0.38"}]
["08017","08","CO","017","Cheyenne","","2104008610","Hydronic heater: outdoor","Hydronic heater",7.309603794362783,"A","CEC Survey",2017,15,"I",18.826030380314492,"TON",8,{"v":2.575519947446845,"d":"2.58"},{"$f":"VLOOKUP(A3799,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.5063448301351157,"d":"2.51"}]
["08019","08","CO","019","Clear Creek","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.0925648038274374,"A","CEC Survey",2017,15,"I",5.7535978060559,"TON",8,{"v":2.7495434289691745,"d":"2.75"},{"$f":"VLOOKUP(A3816,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.7035825260267203,"d":"2.70"}]
["08023","08","CO","023","Costilla","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",32.84244734848,"A","CEC Survey",2017,15,"I",14.626616160467872,"TON",8,{"v":0.4453570711485,"d":"0.45"},{"$f":"VLOOKUP(A3850,cordwood_density!A:D,4,FALSE)","v":1.0577},{"v":0.42106180499999996,"d":"0.42"}]
["08023","08","CO","023","Costilla","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",159.30182600639998,"A","CEC Survey",2017,15,"I",270.6081552213003,"TON",8,{"v":1.6987134548629002,"d":"1.70"},{"$f":"VLOOKUP(A3855,cordwood_density!A:D,4,FALSE)","v":1.0577},{"v":1.606044677,"d":"1.61"}]
["08027","08","CO","027","Custer","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8496956549767428,"A","CEC Survey",2017,15,"I",2.280238188631358,"TON",8,{"v":2.6835940319051894,"d":"2.68"},{"$f":"VLOOKUP(A3876,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.6387355279303732,"d":"2.64"}]
["08031","08","CO","031","Denver","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",102.79254329578414,"A","CEC Survey",2017,15,"I",2.5610046676806522E-4,"TON",8,{"v":2.4914303952100847E-6,"d":"0.00"},{"$f":"VLOOKUP(A3903,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.4245138139451971E-6,"d":"0.00"}]
["08035","08","CO","035","Douglas","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",51.202360990953096,"A","CEC Survey",2017,15,"I",130.096911823691,"TON",8,{"v":2.5408381431215195,"d":"2.54"},{"$f":"VLOOKUP(A3933,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.498365922440039,"d":"2.50"}]
["08037","08","CO","037","Eagle","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",177.77822936885,"A","CEC Survey",2017,15,"I",98.76931764196173,"TON",8,{"v":0.555576000462,"d":"0.56"},{"$f":"VLOOKUP(A3954,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.546289086,"d":"0.55"}]
["08041","08","CO","041","El Paso","","2104008610","Hydronic heater: outdoor","Hydronic heater",750.9988885864299,"A","CEC Survey",2017,15,"I",1802.6873604405394,"TON",8,{"v":2.4003861894305243,"d":"2.40"},{"$f":"VLOOKUP(A3979,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.3602617398530232,"d":"2.36"}]
["08041","08","CO","041","El Paso","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",4708.86597509905,"A","CEC Survey",2017,15,"I",4847.570055369109,"TON",8,{"v":1.0294559414099997,"d":"1.03"},{"$f":"VLOOKUP(A3989,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.01224773,"d":"1.01"}]
["08045","08","CO","045","Garfield","","2104008620","Hydronic heater: indoor","Hydronic heater",95.062164034917,"A","CEC Survey",2017,15,"I",271.7402196554449,"TON",8,{"v":2.858552847120467,"d":"2.86"},{"$f":"VLOOKUP(A4010,cordwood_density!A:D,4,FALSE)","v":1.0582},{"v":2.701335141863983,"d":"2.70"}]
["08047","08","CO","047","Gilpin","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",133.758892908,"A","CEC Survey",2017,15,"I",136.57138764561935,"TON",8,{"v":1.0210266,"d":"1.02"},{"$f":"VLOOKUP(A4032,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9936031529778122,"d":"0.99"}]
["08053","08","CO","053","Hinsdale","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.3066808563338737,"A","CEC Survey",2017,15,"I",0.9273668586917434,"TON",8,{"v":3.0238824482808555,"d":"3.02"},{"$f":"VLOOKUP(A4071,cordwood_density!A:D,4,FALSE)","v":1.0238},{"v":2.9535870758750296,"d":"2.95"}]
["08055","08","CO","055","Huerfano","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",58.60678137030046,"A","CEC Survey",2017,15,"I",25.860767584006464,"TON",8,{"v":0.441258963201,"d":"0.44"},{"$f":"VLOOKUP(A4088,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.433882953,"d":"0.43"}]
["08057","08","CO","057","Jackson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",11.593555646399999,"A","CEC Survey",2017,15,"I",5.473500876404381,"TON",8,{"v":0.4721158066899,"d":"0.47"},{"$f":"VLOOKUP(A4105,cordwood_density!A:D,4,FALSE)","v":1.0587},{"v":0.445939177,"d":"0.45"}]
["08061","08","CO","061","Kiowa","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",20.727474163200004,"A","CEC Survey",2017,15,"I",29.74938836178447,"TON",8,{"v":1.4352635602172001,"d":"1.44"},{"$f":"VLOOKUP(A4141,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.396714247,"d":"1.40"}]
["08063","08","CO","063","Kit Carson","","2104008610","Hydronic heater: outdoor","Hydronic heater",17.710008653993867,"A","CEC Survey",2017,15,"I",44.342267984692995,"TON",8,{"v":2.5037970816966912,"d":"2.50"},{"$f":"VLOOKUP(A4144,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.43654834731091,"d":"2.44"}]
["08065","08","CO","065","Lake","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",45.562900595520006,"A","CEC Survey",2017,15,"I",22.534336806061745,"TON",8,{"v":0.49457643195520007,"d":"0.49"},{"$f":"VLOOKUP(A4165,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.48129275200000005,"d":"0.48"}]
["08069","08","CO","069","Larimer","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2002.31143635002,"A","CEC Survey",2017,15,"I",1076.3399699002898,"TON",8,{"v":0.5375487301128,"d":"0.54"},{"$f":"VLOOKUP(A4194,cordwood_density!A:D,4,FALSE)","v":1.0584},{"v":0.507888067,"d":"0.51"}]
["08073","08","CO","073","Lincoln","","2104008100","Fireplace: general","Fireplace: general",94.151577688,"A","CEC Survey",2017,15,"I",44.193198087071664,"TON",8,{"v":0.469383510848,"d":"0.47"},{"$f":"VLOOKUP(A4222,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.45677648,"d":"0.46"}]
["08075","08","CO","075","Logan","","2104009000","Wax Log; Total: All Combustor Types",null,154.3503011738653,"A","CEC Survey",2017,15,"I",120.46954570451527,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A4243,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["08079","08","CO","079","Mineral","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",10.504070942400002,"A","CEC Survey",2017,15,"I",5.873899030142074,"TON",8,{"v":0.5592021476580001,"d":"0.56"},{"$f":"VLOOKUP(A4270,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5441827050000001,"d":"0.54"}]
["08081","08","CO","081","Moffat","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.7094463210316695,"A","CEC Survey",2017,15,"I",7.394908610320254,"TON",8,{"v":2.72930618810138,"d":"2.73"},{"$f":"VLOOKUP(A4278,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.683683567454651,"d":"2.68"}]
["08083","08","CO","083","Montezuma","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",247.301074484,"A","CEC Survey",2017,15,"I",111.98572664014807,"TON",8,{"v":0.45283154096200007,"d":"0.45"},{"$f":"VLOOKUP(A4299,cordwood_density!A:D,4,FALSE)","v":1.0526},{"v":0.43020287000000007,"d":"0.43"}]
["08087","08","CO","087","Morgan","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.9380227127886815,"A","CEC Survey",2017,15,"I",15.881380029434743,"TON",8,{"v":2.674523287900384,"d":"2.67"},{"$f":"VLOOKUP(A4323,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.6026890695799767,"d":"2.60"}]
["08091","08","CO","091","Ouray","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",36.76512394688,"A","CEC Survey",2017,15,"I",20.098706086631683,"TON",8,{"v":0.5466785890800001,"d":"0.55"},{"$f":"VLOOKUP(A4360,cordwood_density!A:D,4,FALSE)","v":1.0335},{"v":0.52895848,"d":"0.53"}]
["08093","08","CO","093","Park","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",410.534258688,"A","CEC Survey",2017,15,"I",332.2162144867353,"TON",8,{"v":0.809228968,"d":"0.81"},{"$f":"VLOOKUP(A4377,cordwood_density!A:D,4,FALSE)","v":1.0579},{"v":0.7649389999054731,"d":"0.76"}]
["08097","08","CO","097","Pitkin","","2104008610","Hydronic heater: outdoor","Hydronic heater",49.1135210677915,"A","CEC Survey",2017,15,"I",141.83271101192952,"TON",8,{"v":2.8878546666641456,"d":"2.89"},{"$f":"VLOOKUP(A4399,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.8395817764642537,"d":"2.84"}]
["08099","08","CO","099","Prowers","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.5924761394615705,"A","CEC Survey",2017,15,"I",1.437701534048812,"TON",8,{"v":2.426598200824364,"d":"2.43"},{"$f":"VLOOKUP(A4416,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.3614229280112533,"d":"2.36"}]
["08101","08","CO","101","Pueblo","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",695.1944603281199,"A","CEC Survey",2017,15,"I",264.5117188685034,"TON",8,{"v":0.3804859416509999,"d":"0.38"},{"$f":"VLOOKUP(A4433,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.374125803,"d":"0.37"}]
["08105","08","CO","105","Rio Grande","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",110.4412780075,"A","CEC Survey",2017,15,"I",50.47868361210623,"TON",8,{"v":0.45706355923080005,"d":"0.46"},{"$f":"VLOOKUP(A4464,cordwood_density!A:D,4,FALSE)","v":1.0182},{"v":0.44889369400000007,"d":"0.45"}]
["08109","08","CO","109","Saguache","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",71.00189839704001,"A","CEC Survey",2017,15,"I",31.58311870643974,"TON",8,{"v":0.4448207642256,"d":"0.44"},{"$f":"VLOOKUP(A4494,cordwood_density!A:D,4,FALSE)","v":1.0258},{"v":0.433633032,"d":"0.43"}]
["08111","08","CO","111","San Juan","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,33.587335965,"A","CEC Survey",2017,15,"I",9.221367851480576,"TON",8,{"v":0.2745489508632,"d":"0.27"},{"$f":"VLOOKUP(A4511,cordwood_density!A:D,4,FALSE)","v":1.0182},{"v":0.26964147600000005,"d":"0.27"}]
["08115","08","CO","115","Sedgwick","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",9.449695608894888,"A","CEC Survey",2017,15,"I",23.88667095496986,"TON",8,{"v":2.527771469430784,"d":"2.53"},{"$f":"VLOOKUP(A4532,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.4598788141599686,"d":"2.46"}]
["08117","08","CO","117","Summit","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",146.99726091525298,"A","CEC Survey",2017,15,"I",185.5481081219678,"TON",8,{"v":1.262255547938,"d":"1.26"},{"$f":"VLOOKUP(A4561,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.228353005,"d":"1.23"}]
["08119","08","CO","119","Teller","","2104008100","Fireplace: general","Fireplace: general",1089.134981924,"A","CEC Survey",2017,15,"I",430.7792768712006,"TON",8,{"v":0.395524231634,"d":"0.40"},{"$f":"VLOOKUP(A4567,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.384900965,"d":"0.38"}]
["08125","08","CO","125","Yuma","","2104008620","Hydronic heater: indoor","Hydronic heater",18.202597746535364,"A","CEC Survey",2017,15,"I",45.90741633908923,"TON",8,{"v":2.5220255360434547,"d":"2.52"},{"$f":"VLOOKUP(A4610,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.4542872090730388,"d":"2.45"}]
["08125","08","CO","125","Yuma","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",70.03143562815107,"A","CEC Survey",2017,15,"I",25.362643431950563,"TON",8,{"v":0.36216083826440004,"d":"0.36"},{"$f":"VLOOKUP(A4614,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.352433669,"d":"0.35"}]
["09003","09","CT","003","Hartford","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",3782.3000177271997,"A","CEC Survey",2017,15,"I",3918.047908959994,"TON",8,{"v":1.0358903023547998,"d":"1.04"},{"$f":"VLOOKUP(A4649,cordwood_density!A:D,4,FALSE)","v":1.3604},{"v":0.7614600869999999,"d":"0.76"}]
["09005","09","CT","005","Litchfield","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",4003.418968421616,"A","CEC Survey",2017,15,"I",6170.075396489802,"TON",8,{"v":1.541201519291,"d":"1.54"},{"$f":"VLOOKUP(A4666,cordwood_density!A:D,4,FALSE)","v":1.4219},{"v":1.08390289,"d":"1.08"}]
["09009","09","CT","009","New Haven","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",4548.6669274653605,"A","CEC Survey",2017,15,"I",3227.763090707925,"TON",8,{"v":0.7096063840635,"d":"0.71"},{"$f":"VLOOKUP(A4690,cordwood_density!A:D,4,FALSE)","v":1.4189},{"v":0.500110215,"d":"0.50"}]
["09011","09","CT","011","New London","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",2465.0368654605004,"A","CEC Survey",2017,15,"I",1847.9143122539865,"TON",8,{"v":0.7496497671683999,"d":"0.75"},{"$f":"VLOOKUP(A4705,cordwood_density!A:D,4,FALSE)","v":1.3539},{"v":0.5536965559999999,"d":"0.55"}]
["10001","10","DE","001","Kent","","2104008610","Hydronic heater: outdoor","Hydronic heater",206.55513513247152,"A","CEC Survey",2017,15,"I",562.5883426357507,"TON",8,{"v":2.723671538230903,"d":"2.72"},{"$f":"VLOOKUP(A4744,cordwood_density!A:D,4,FALSE)","v":1.252},{"v":2.1754565001844273,"d":"2.18"}]
["10003","10","DE","003","New Castle","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,12179.020651632,"A","CEC Survey",2017,15,"I",6845.283030406797,"TON",8,{"v":0.5620552937883,"d":"0.56"},{"$f":"VLOOKUP(A4766,cordwood_density!A:D,4,FALSE)","v":1.2987},{"v":0.432783009,"d":"0.43"}]
["10005","10","DE","005","Sussex","","2104009000","Wax Log; Total: All Combustor Types",null,839.4223350228515,"A","CEC Survey",2017,15,"I",117.51912690319922,"TON",8,0.14,{"$f":"VLOOKUP(A4783,cordwood_density!A:D,4,FALSE)","v":1.1867},{"v":0.11797421420746608,"d":"0.12"}]
["11001","11","DC","001","District of Columbia","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1206.4982267421,"A","CEC Survey",2017,15,"I",44.165457384162465,"TON",8,{"v":0.036606317693000004,"d":"0.04"},{"$f":"VLOOKUP(A4800,cordwood_density!A:D,4,FALSE)","v":1.2934},{"v":0.028302395,"d":"0.03"}]
["12003","12","FL","003","Baker","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",259.36670633058725,"A","CEC Survey",2017,15,"I",314.7895940534028,"TON",8,{"v":1.2136854359871998,"d":"1.21"},{"$f":"VLOOKUP(A4831,cordwood_density!A:D,4,FALSE)","v":1.3382},{"v":0.9069536959999999,"d":"0.91"}]
["12005","12","FL","005","Bay","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1640.92694153943,"A","CEC Survey",2017,15,"I",873.7526228217769,"TON",8,{"v":0.5324750302424,"d":"0.53"},{"$f":"VLOOKUP(A4839,cordwood_density!A:D,4,FALSE)","v":1.2952},{"v":0.411114137,"d":"0.41"}]
["12011","12","FL","011","Broward","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",30.994788514738907,"A","CEC Survey",2017,15,"I",18.233530110091216,"TON",8,{"v":0.5882772873710899,"d":"0.59"},{"$f":"VLOOKUP(A4878,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.48933396054823647,"d":"0.49"}]
["12011","12","FL","011","Broward","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",9954.24893143776,"A","CEC Survey",2017,15,"I",3587.589437504114,"TON",8,{"v":0.3604078481675999,"d":"0.36"},{"$f":"VLOOKUP(A4884,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.2997902579999999,"d":"0.30"}]
["12015","12","FL","015","Charlotte","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1739.740508132,"A","CEC Survey",2017,15,"I",151.54685759245245,"TON",8,{"v":0.087108886,"d":"0.09"},{"$f":"VLOOKUP(A4917,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.08565278859390364,"d":"0.09"}]
["12019","12","FL","019","Clay","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.950110713786193,"A","CEC Survey",2017,15,"I",20.852341547415335,"TON",8,{"v":1.9043041748575409,"d":"1.90"},{"$f":"VLOOKUP(A4938,cordwood_density!A:D,4,FALSE)","v":1.3009},{"v":1.4638359403932208,"d":"1.46"}]
["12021","12","FL","021","Collier","","2104008620","Hydronic heater: indoor","Hydronic heater",59.53292186547298,"A","CEC Survey",2017,15,"I",104.4678631684224,"TON",8,{"v":1.754791464871979,"d":"1.75"},{"$f":"VLOOKUP(A4955,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.359671055998744,"d":"1.36"}]
["12023","12","FL","023","Columbia","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",730.7509794261601,"A","CEC Survey",2017,15,"I",836.1505007906802,"TON",8,{"v":1.1442345263051,"d":"1.14"},{"$f":"VLOOKUP(A4981,cordwood_density!A:D,4,FALSE)","v":1.2721},{"v":0.8994847309999999,"d":"0.90"}]
["12027","12","FL","027","De Soto","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",295.50415196032,"A","CEC Survey",2017,15,"I",311.22799198851453,"TON",8,{"v":1.0532102169255,"d":"1.05"},{"$f":"VLOOKUP(A4994,cordwood_density!A:D,4,FALSE)","v":1.3305},{"v":0.7915897909999999,"d":"0.79"}]
["12033","12","FL","033","Escambia","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",2418.3981704318803,"A","CEC Survey",2017,15,"I",1287.8943633475772,"TON",8,{"v":0.5325402487868999,"d":"0.53"},{"$f":"VLOOKUP(A5033,cordwood_density!A:D,4,FALSE)","v":1.2627},{"v":0.42174724699999994,"d":"0.42"}]
["12037","12","FL","037","Franklin","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",12.16442297121147,"A","CEC Survey",2017,15,"I",22.255963177472868,"TON",8,{"v":1.8295946490963202,"d":"1.83"},{"$f":"VLOOKUP(A5057,cordwood_density!A:D,4,FALSE)","v":1.2149},{"v":1.505963164948819,"d":"1.51"}]
["12039","12","FL","039","Gadsden","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",65.35615475952198,"A","CEC Survey",2017,15,"I",123.80733596652448,"TON",8,{"v":1.894348534152195,"d":"1.89"},{"$f":"VLOOKUP(A5072,cordwood_density!A:D,4,FALSE)","v":1.2553},{"v":1.5090803267363937,"d":"1.51"}]
["12041","12","FL","041","Gilchrist","","2104008610","Hydronic heater: outdoor","Hydronic heater",18.241043816853207,"A","CEC Survey",2017,15,"I",34.967578909878604,"TON",8,{"v":1.916972474874024,"d":"1.92"},{"$f":"VLOOKUP(A5089,cordwood_density!A:D,4,FALSE)","v":1.216},{"v":1.5764576273635067,"d":"1.58"}]
["12045","12","FL","045","Gulf","","2104008100","Fireplace: general","Fireplace: general",453.99593691,"A","CEC Survey",2017,15,"I",161.9828158500669,"TON",8,{"v":0.3567935364192,"d":"0.36"},{"$f":"VLOOKUP(A5122,cordwood_density!A:D,4,FALSE)","v":1.2249},{"v":0.291283808,"d":"0.29"}]
["12045","12","FL","045","Gulf","","2104009000","Wax Log; Total: All Combustor Types",null,76.05193767538053,"A","CEC Survey",2017,15,"I",17.806215087393497,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A5128,cordwood_density!A:D,4,FALSE)","v":1.2249},{"v":0.19114401175606172,"d":"0.19"}]
["12051","12","FL","051","Hendry","","2104008100","Fireplace: general","Fireplace: general",552.8435278979999,"A","CEC Survey",2017,15,"I",199.4258394123527,"TON",8,{"v":0.36072745604999995,"d":"0.36"},{"$f":"VLOOKUP(A5167,cordwood_density!A:D,4,FALSE)","v":1.3173},{"v":0.2738385,"d":"0.27"}]
["12051","12","FL","051","Hendry","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",376.68594987856,"A","CEC Survey",2017,15,"I",384.66325096909543,"TON",8,{"v":1.0211775912881997,"d":"1.02"},{"$f":"VLOOKUP(A5175,cordwood_density!A:D,4,FALSE)","v":1.3173},{"v":0.7752050339999998,"d":"0.78"}]
["12055","12","FL","055","Highlands","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",830.710987176,"A","CEC Survey",2017,15,"I",795.1825824155896,"TON",8,{"v":0.9572313291760001,"d":"0.96"},{"$f":"VLOOKUP(A5206,cordwood_density!A:D,4,FALSE)","v":1.348},{"v":0.710112262,"d":"0.71"}]
["12059","12","FL","059","Holmes","","2104008100","Fireplace: general","Fireplace: general",538.18364994,"A","CEC Survey",2017,15,"I",225.38979206503637,"TON",8,{"v":0.4187971747008,"d":"0.42"},{"$f":"VLOOKUP(A5227,cordwood_density!A:D,4,FALSE)","v":1.4744},{"v":0.28404583200000005,"d":"0.28"}]
["12061","12","FL","061","Indian River","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",944.8280322482401,"A","CEC Survey",2017,15,"I",695.1462524467352,"TON",8,{"$f":"P5251/J5251","v":{"v":0.7357383870084999,"d":"0.74"}},{"$f":"VLOOKUP(A5251,cordwood_density!A:D,4,FALSE)","v":1.1959},{"$f":"S5251/T5251","v":{"v":0.615217315,"d":"0.62"}}]
["12063","12","FL","063","Jackson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",595.338701347,"A","CEC Survey",2017,15,"I",131.83885440853584,"TON",8,{"v":0.221451846,"d":"0.22"},{"$f":"VLOOKUP(A5262,cordwood_density!A:D,4,FALSE)","v":1.3486},{"v":0.16420869494290374,"d":"0.16"}]
["12067","12","FL","067","Lafayette","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.678081757486354,"A","CEC Survey",2017,15,"I",1.4021176041112247,"TON",8,{"v":2.0677707203167777,"d":"2.07"},{"$f":"VLOOKUP(A5283,cordwood_density!A:D,4,FALSE)","v":1.3064},{"v":1.5828006126123528,"d":"1.58"}]
["12069","12","FL","069","Lake","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3978.60621120833,"A","CEC Survey",2017,15,"I",1953.8109120882173,"TON",8,{"v":0.4910792394040001,"d":"0.49"},{"$f":"VLOOKUP(A5304,cordwood_density!A:D,4,FALSE)","v":1.247},{"v":0.39380853200000004,"d":"0.39"}]
["12073","12","FL","073","Leon","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2790.4930696832403,"A","CEC Survey",2017,15,"I",2630.954080487188,"TON",8,{"v":0.9428276705183998,"d":"0.94"},{"$f":"VLOOKUP(A5340,cordwood_density!A:D,4,FALSE)","v":1.3656},{"v":0.6904127639999998,"d":"0.69"}]
["12077","12","FL","077","Liberty","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.283739860637964,"A","CEC Survey",2017,15,"I",0.6190206014959992,"TON",8,{"v":2.181648359536746,"d":"2.18"},{"$f":"VLOOKUP(A5361,cordwood_density!A:D,4,FALSE)","v":1.3486},{"v":1.6177134506427007,"d":"1.62"}]
["12079","12","FL","079","Madison","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",203.97300924022,"A","CEC Survey",2017,15,"I",123.64170095416065,"TON",8,{"v":0.6061669699080001,"d":"0.61"},{"$f":"VLOOKUP(A5378,cordwood_density!A:D,4,FALSE)","v":1.228},{"v":0.4936213110000001,"d":"0.49"}]
["12083","12","FL","083","Marion","","2104009000","Wax Log; Total: All Combustor Types",null,1935.3674118875356,"A","CEC Survey",2017,15,"I",453.132023490276,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A5413,cordwood_density!A:D,4,FALSE)","v":1.3303},{"v":0.1759996241449297,"d":"0.18"}]
["12085","12","FL","085","Martin","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",51.21599218090656,"A","CEC Survey",2017,15,"I",78.1479336947426,"TON",8,{"v":1.5258502347998315,"d":"1.53"},{"$f":"VLOOKUP(A5417,cordwood_density!A:D,4,FALSE)","v":1.1096},{"v":1.3751353954576708,"d":"1.38"}]
["12087","12","FL","087","Monroe","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3032.931237924,"A","CEC Survey",2017,15,"I",721.7058527354606,"TON",8,{"v":0.23795654966100002,"d":"0.24"},{"$f":"VLOOKUP(A5456,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.184376685,"d":"0.18"}]
["12089","12","FL","089","Nassau","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.045884391143683,"A","CEC Survey",2017,15,"I",4.097746598194986,"TON",8,{"v":2.0029218737546937,"d":"2.00"},{"$f":"VLOOKUP(A5466,cordwood_density!A:D,4,FALSE)","v":1.349},{"v":1.4847456439990316,"d":"1.48"}]
["12093","12","FL","093","Okeechobee","","2104008620","Hydronic heater: indoor","Hydronic heater",11.02133958260456,"A","CEC Survey",2017,15,"I",20.778726865280035,"TON",8,{"v":1.8853177247234054,"d":"1.89"},{"$f":"VLOOKUP(A5495,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.4608071631205684,"d":"1.46"}]
["12095","12","FL","095","Orange","","2104008100","Fireplace: general","Fireplace: general",25950.729225781823,"A","CEC Survey",2017,15,"I",5247.646239353244,"TON",8,{"v":0.20221575254000004,"d":"0.20"},{"$f":"VLOOKUP(A5512,cordwood_density!A:D,4,FALSE)","v":1.27},{"v":0.15922500200000003,"d":"0.16"}]
["12099","12","FL","099","Palm Beach","","2104008100","Fireplace: general","Fireplace: general",19894.029765992997,"A","CEC Survey",2017,15,"I",5090.172895840415,"TON",8,{"v":0.2558643450178,"d":"0.26"},{"$f":"VLOOKUP(A5542,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.212830099,"d":"0.21"}]
["12099","12","FL","099","Palm Beach","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",5694.19102322532,"A","CEC Survey",2017,15,"I",3588.73701370725,"TON",8,{"v":0.6302452796314,"d":"0.63"},{"$f":"VLOOKUP(A5551,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.524243287,"d":"0.52"}]
["12103","12","FL","103","Pinellas","","2104008100","Fireplace: general","Fireplace: general",16342.068109072,"A","CEC Survey",2017,15,"I",1798.8669892692196,"TON",8,{"v":0.11007584702640001,"d":"0.11"},{"$f":"VLOOKUP(A5572,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.085290444,"d":"0.09"}]
["12105","12","FL","105","Polk","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6155.25406680772,"A","CEC Survey",2017,15,"I",5399.225870711693,"TON",8,{"v":0.8771735190959999,"d":"0.88"},{"$f":"VLOOKUP(A5595,cordwood_density!A:D,4,FALSE)","v":1.332},{"v":0.6585386779999999,"d":"0.66"}]
["12111","12","FL","111","St Lucie","","2104008610","Hydronic heater: outdoor","Hydronic heater",115.46292590391549,"A","CEC Survey",2017,15,"I",186.1883231931451,"TON",8,{"v":1.6125377192336612,"d":"1.61"},{"$f":"VLOOKUP(A5629,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":1.3413223417348705,"d":"1.34"}]
["12113","12","FL","113","Santa Rosa","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1500.52601658064,"A","CEC Survey",2017,15,"I",936.9834078307217,"TON",8,{"v":0.6244366292068,"d":"0.62"},{"$f":"VLOOKUP(A5650,cordwood_density!A:D,4,FALSE)","v":1.4062},{"v":0.44405961400000005,"d":"0.44"}]
["12115","12","FL","115","Sarasota","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2547.66144394888,"A","CEC Survey",2017,15,"I",2074.360250248547,"TON",8,{"v":0.8142213146788,"d":"0.81"},{"$f":"VLOOKUP(A5671,cordwood_density!A:D,4,FALSE)","v":1.4639},{"v":0.556200092,"d":"0.56"}]
["12119","12","FL","119","Sumter","","2104008610","Hydronic heater: outdoor","Hydronic heater",87.65969398032783,"A","CEC Survey",2017,15,"I",166.31438456707437,"TON",8,{"v":1.8972731595937107,"d":"1.90"},{"$f":"VLOOKUP(A5689,cordwood_density!A:D,4,FALSE)","v":1.3906},{"v":1.364355788575946,"d":"1.36"}]
["12121","12","FL","121","Suwannee","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0876772345960393,"A","CEC Survey",2017,15,"I",2.4017442546830434,"TON",8,{"v":2.208140593817839,"d":"2.21"},{"$f":"VLOOKUP(A5706,cordwood_density!A:D,4,FALSE)","v":1.4035},{"v":1.5733100062827496,"d":"1.57"}]
["12127","12","FL","127","Volusia","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",253.12765465111556,"A","CEC Survey",2017,15,"I",422.84097495215656,"TON",8,{"v":1.6704653449855407,"d":"1.67"},{"$f":"VLOOKUP(A5747,cordwood_density!A:D,4,FALSE)","v":1.2225},{"v":1.3664338200290722,"d":"1.37"}]
["12129","12","FL","129","Wakulla","","2104008100","Fireplace: general","Fireplace: general",916.973950875,"A","CEC Survey",2017,15,"I",347.5897813580829,"TON",8,{"v":0.3790617836269,"d":"0.38"},{"$f":"VLOOKUP(A5767,cordwood_density!A:D,4,FALSE)","v":1.3849},{"v":0.273710581,"d":"0.27"}]
["12131","12","FL","131","Walton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",740.0019504144899,"A","CEC Survey",2017,15,"I",443.33942205760997,"TON",8,{"v":0.5991057480447,"d":"0.60"},{"$f":"VLOOKUP(A5784,cordwood_density!A:D,4,FALSE)","v":1.3449},{"v":0.44546490299999997,"d":"0.45"}]
["12133","12","FL","133","Washington","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1185.255640074,"A","CEC Survey",2017,15,"I",295.1692073019526,"TON",8,{"v":0.2490342144953,"d":"0.25"},{"$f":"VLOOKUP(A5801,cordwood_density!A:D,4,FALSE)","v":1.3141},{"v":0.189509333,"d":"0.19"}]
["13003","13","GA","003","Atkinson","","2104009000","Wax Log; Total: All Combustor Types",null,40.71902610644984,"A","CEC Survey",2017,15,"I",9.533639236063145,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A5833,cordwood_density!A:D,4,FALSE)","v":1.2494},{"v":0.18739578997919,"d":"0.19"}]
["13005","13","GA","005","Bacon","","2104008620","Hydronic heater: indoor","Hydronic heater",8.35659648519869,"A","CEC Survey",2017,15,"I",16.91782824553658,"TON",8,{"v":2.024487873203122,"d":"2.02"},{"$f":"VLOOKUP(A5840,cordwood_density!A:D,4,FALSE)","v":1.4733},{"v":1.374117880406653,"d":"1.37"}]
["13007","13","GA","007","Baker","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,191.34346163499998,"A","CEC Survey",2017,15,"I",44.240067773181416,"TON",8,{"v":0.23120762734800002,"d":"0.23"},{"$f":"VLOOKUP(A5861,cordwood_density!A:D,4,FALSE)","v":1.3518},{"v":0.17103686,"d":"0.17"}]
["13011","13","GA","011","Banks","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2350793793738835,"A","CEC Survey",2017,15,"I",2.1286609882628698,"TON",8,{"v":1.7235013585458632,"d":"1.72"},{"$f":"VLOOKUP(A5886,cordwood_density!A:D,4,FALSE)","v":1.1511},{"v":1.4972646673146235,"d":"1.50"}]
["13015","13","GA","015","Bartow","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",867.6494506112,"A","CEC Survey",2017,15,"I",538.2730668179313,"TON",8,{"v":0.620380807524,"d":"0.62"},{"$f":"VLOOKUP(A5918,cordwood_density!A:D,4,FALSE)","v":1.332},{"v":0.46575135700000003,"d":"0.47"}]
["13017","13","GA","017","Ben Hill","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",179.00772604731998,"A","CEC Survey",2017,15,"I",163.81515603920553,"TON",8,{"v":0.915128970444,"d":"0.92"},{"$f":"VLOOKUP(A5939,cordwood_density!A:D,4,FALSE)","v":1.2402},{"v":0.73788822,"d":"0.74"}]
["13021","13","GA","021","Bibb","","2104008100","Fireplace: general","Fireplace: general",7449.331485428999,"A","CEC Survey",2017,15,"I",1546.9253391080717,"TON",8,{"v":0.20765961913949998,"d":"0.21"},{"$f":"VLOOKUP(A5962,cordwood_density!A:D,4,FALSE)","v":1.2013},{"v":0.172862415,"d":"0.17"}]
["13023","13","GA","023","Bleckley","","2104008610","Hydronic heater: outdoor","Hydronic heater",15.373530562931242,"A","CEC Survey",2017,15,"I",28.290606689815522,"TON",8,{"v":1.8402153346629446,"d":"1.84"},{"$f":"VLOOKUP(A5974,cordwood_density!A:D,4,FALSE)","v":1.3273},{"v":1.386435119914823,"d":"1.39"}]
["13025","13","GA","025","Brantley","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",198.4860970255717,"A","CEC Survey",2017,15,"I",117.49875146432409,"TON",8,{"v":0.5919747187592,"d":"0.59"},{"$f":"VLOOKUP(A5995,cordwood_density!A:D,4,FALSE)","v":1.3064},{"v":0.45313435300000005,"d":"0.45"}]
["13031","13","GA","031","Bulloch","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",617.5040296878399,"A","CEC Survey",2017,15,"I",316.6045352788503,"TON",8,{"v":0.5127165492975,"d":"0.51"},{"$f":"VLOOKUP(A6038,cordwood_density!A:D,4,FALSE)","v":1.2087},{"v":0.424188425,"d":"0.42"}]
["13033","13","GA","033","Burke","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1071.509369584,"A","CEC Survey",2017,15,"I",231.62076622618463,"TON",8,{"v":0.2161630806048,"d":"0.22"},{"$f":"VLOOKUP(A6056,cordwood_density!A:D,4,FALSE)","v":1.2744},{"v":0.169619492,"d":"0.17"}]
["13035","13","GA","035","Butts","","2104009000","Wax Log; Total: All Combustor Types",null,74.50394804115949,"A","CEC Survey",2017,15,"I",17.443780713957164,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A6073,cordwood_density!A:D,4,FALSE)","v":1.4076},{"v":0.16633439897698207,"d":"0.17"}]
["13037","13","GA","037","Calhoun","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",65.0527172148,"A","CEC Survey",2017,15,"I",67.01683152704383,"TON",8,{"v":1.0301926559924999,"d":"1.03"},{"$f":"VLOOKUP(A6091,cordwood_density!A:D,4,FALSE)","v":1.1965},{"v":0.8610051449999999,"d":"0.86"}]
["13043","13","GA","043","Candler","","2104008100","Fireplace: general","Fireplace: general",243.537662375,"A","CEC Survey",2017,15,"I",73.63003850417127,"TON",8,{"v":0.30233532582239997,"d":"0.30"},{"$f":"VLOOKUP(A6112,cordwood_density!A:D,4,FALSE)","v":1.2279},{"v":0.24622145599999998,"d":"0.25"}]
["13045","13","GA","045","Carroll","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1295.920992497963,"A","CEC Survey",2017,15,"I",847.508464606861,"TON",8,{"v":0.6539815849214999,"d":"0.65"},{"$f":"VLOOKUP(A6129,cordwood_density!A:D,4,FALSE)","v":1.3521},{"v":0.4836784149999999,"d":"0.48"}]
["13051","13","GA","051","Chatham","","2104008100","Fireplace: general","Fireplace: general",7038.862940403,"A","CEC Survey",2017,15,"I",1701.7990740830141,"TON",8,{"v":0.24177187260099997,"d":"0.24"},{"$f":"VLOOKUP(A6172,cordwood_density!A:D,4,FALSE)","v":1.277},{"v":0.189328013,"d":"0.19"}]
["13051","13","GA","051","Chatham","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2264.538707757,"A","CEC Survey",2017,15,"I",255.32822710153275,"TON",8,{"v":0.112750657,"d":"0.11"},{"$f":"VLOOKUP(A6177,cordwood_density!A:D,4,FALSE)","v":1.277},{"v":0.08829338841033674,"d":"0.09"}]
["13055","13","GA","055","Chattooga","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",320.45061769936785,"A","CEC Survey",2017,15,"I",109.17833683113864,"TON",8,{"v":0.340702532,"d":"0.34"},{"$f":"VLOOKUP(A6207,cordwood_density!A:D,4,FALSE)","v":1.3202},{"v":0.2580688774428117,"d":"0.26"}]
["13059","13","GA","059","Clarke","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.956003226595583,"A","CEC Survey",2017,15,"I",9.720769790261688,"TON",8,{"v":1.221815717440484,"d":"1.22"},{"$f":"VLOOKUP(A6228,cordwood_density!A:D,4,FALSE)","v":1.1936},{"v":1.0236391734588506,"d":"1.02"}]
["13061","13","GA","061","Clay","","2104009000","Wax Log; Total: All Combustor Types",null,16.574869891858192,"A","CEC Survey",2017,15,"I",3.8807124099815096,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A6253,cordwood_density!A:D,4,FALSE)","v":1.3256},{"v":0.17662364212432108,"d":"0.18"}]
["13063","13","GA","063","Clayton","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1323.6373560624554,"A","CEC Survey",2017,15,"I",741.7222780968107,"TON",8,{"v":0.5603666855575,"d":"0.56"},{"$f":"VLOOKUP(A6263,cordwood_density!A:D,4,FALSE)","v":1.2725},{"v":0.440366747,"d":"0.44"}]
["13069","13","GA","069","Coffee","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2978494872486022,"A","CEC Survey",2017,15,"I",2.1694829199221495,"TON",8,{"v":1.6715982409650454,"d":"1.67"},{"$f":"VLOOKUP(A6306,cordwood_density!A:D,4,FALSE)","v":1.2095},{"v":1.3820572475940847,"d":"1.38"}]
["13071","13","GA","071","Colquitt","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",482.83053694440997,"A","CEC Survey",2017,15,"I",470.1730306330227,"TON",8,{"v":0.973784785048,"d":"0.97"},{"$f":"VLOOKUP(A6329,cordwood_density!A:D,4,FALSE)","v":1.258},{"v":0.7740737560000001,"d":"0.77"}]
["13073","13","GA","073","Columbia","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1430.2509928218299,"A","CEC Survey",2017,15,"I",1087.4896772366626,"TON",8,{"v":0.7603488357600001,"d":"0.76"},{"$f":"VLOOKUP(A6345,cordwood_density!A:D,4,FALSE)","v":1.203},{"v":0.6320439200000001,"d":"0.63"}]
["13077","13","GA","077","Coweta","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",189.94861999114414,"A","CEC Survey",2017,15,"I",274.43301216708545,"TON",8,{"v":1.4447749721997463,"d":"1.44"},{"$f":"VLOOKUP(A6362,cordwood_density!A:D,4,FALSE)","v":1.1208},{"v":1.2890568988220434,"d":"1.29"}]
["13079","13","GA","079","Crawford","","2104008100","Fireplace: general","Fireplace: general",371.93218982499997,"A","CEC Survey",2017,15,"I",117.60845147359024,"TON",8,{"v":0.31620939163379996,"d":"0.32"},{"$f":"VLOOKUP(A6382,cordwood_density!A:D,4,FALSE)","v":1.2319},{"v":0.256684302,"d":"0.26"}]
["13081","13","GA","081","Crisp","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1070.741915472,"A","CEC Survey",2017,15,"I",260.88789730381455,"TON",8,{"v":0.2436515219345,"d":"0.24"},{"$f":"VLOOKUP(A6401,cordwood_density!A:D,4,FALSE)","v":1.4435},{"v":0.16879218699999998,"d":"0.17"}]
["13087","13","GA","087","Decatur","","2104008620","Hydronic heater: indoor","Hydronic heater",20.009226164887483,"A","CEC Survey",2017,15,"I",36.68495917556779,"TON",8,{"v":1.833402195230476,"d":"1.83"},{"$f":"VLOOKUP(A6440,cordwood_density!A:D,4,FALSE)","v":1.3515},{"v":1.3565684019463382,"d":"1.36"}]
["13087","13","GA","087","Decatur","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",320.46808655399997,"A","CEC Survey",2017,15,"I",59.929117541222176,"TON",8,{"v":0.187004947,"d":"0.19"},{"$f":"VLOOKUP(A6447,cordwood_density!A:D,4,FALSE)","v":1.3515},{"v":0.13836844025157233,"d":"0.14"}]
["13091","13","GA","091","Dodge","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",291.79103125526,"A","CEC Survey",2017,15,"I",305.6299211920493,"TON",8,{"v":1.0474273999350001,"d":"1.05"},{"$f":"VLOOKUP(A6479,cordwood_density!A:D,4,FALSE)","v":1.2411},{"v":0.84395085,"d":"0.84"}]
["13093","13","GA","093","Dooly","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",152.9766345012236,"A","CEC Survey",2017,15,"I",157.4530287781731,"TON",8,{"v":1.0292619476925,"d":"1.03"},{"$f":"VLOOKUP(A6496,cordwood_density!A:D,4,FALSE)","v":1.3275},{"v":0.775338567,"d":"0.78"}]
["13097","13","GA","097","Douglas","","2104009000","Wax Log; Total: All Combustor Types",null,448.02287195345707,"A","CEC Survey",2017,15,"I",153.86393488638583,"TON",8,{"v":0.34342875000000006,"d":"0.34"},{"$f":"VLOOKUP(A6523,cordwood_density!A:D,4,FALSE)","v":1.1679},{"v":0.2940566401232983,"d":"0.29"}]
["13099","13","GA","099","Early","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",98.32797805824,"A","CEC Survey",2017,15,"I",48.63074292917522,"TON",8,{"v":0.4945768629592999,"d":"0.49"},{"$f":"VLOOKUP(A6535,cordwood_density!A:D,4,FALSE)","v":1.2703},{"v":0.38933863099999994,"d":"0.39"}]
["13105","13","GA","105","Elbert","","2104008610","Hydronic heater: outdoor","Hydronic heater",37.20473912798648,"A","CEC Survey",2017,15,"I",63.67715123820078,"TON",8,{"v":1.7115333350180915,"d":"1.71"},{"$f":"VLOOKUP(A6574,cordwood_density!A:D,4,FALSE)","v":1.2018},{"v":1.4241415668314956,"d":"1.42"}]
["13107","13","GA","107","Emanuel","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",221.14539939020767,"A","CEC Survey",2017,15,"I",119.05394189207432,"TON",8,{"$f":"P6595/J6595","v":{"v":0.5383514295136,"d":"0.54"}},{"$f":"VLOOKUP(A6595,cordwood_density!A:D,4,FALSE)","v":1.1668},{"$f":"S6595/T6595","v":{"v":0.46139135200000003,"d":"0.46"}}]
["13107","13","GA","107","Emanuel","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",290.7529761216671,"A","CEC Survey",2017,15,"I",71.2872266824775,"TON",8,{"v":0.24518141699999998,"d":"0.25"},{"$f":"VLOOKUP(A6597,cordwood_density!A:D,4,FALSE)","v":1.1668},{"v":0.21013148525882755,"d":"0.21"}]
["13113","13","GA","113","Fayette","","2104008610","Hydronic heater: outdoor","Hydronic heater",113.34401181670657,"A","CEC Survey",2017,15,"I",167.83429395879872,"TON",8,{"v":1.4807513098284426,"d":"1.48"},{"$f":"VLOOKUP(A6634,cordwood_density!A:D,4,FALSE)","v":1.2267},{"v":1.2071014182998636,"d":"1.21"}]
["13115","13","GA","115","Floyd","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.124488370021011,"A","CEC Survey",2017,15,"I",7.307452632839528,"TON",8,{"v":1.77172341809811,"d":"1.77"},{"$f":"VLOOKUP(A6651,cordwood_density!A:D,4,FALSE)","v":1.3228},{"v":1.3393736151331344,"d":"1.34"}]
["13117","13","GA","117","Forsyth","","2104009000","Wax Log; Total: All Combustor Types",null,651.9488650893366,"A","CEC Survey",2017,15,"I",223.8979838015495,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A6673,cordwood_density!A:D,4,FALSE)","v":1.2712},{"v":0.2701610682819383,"d":"0.27"}]
["13119","13","GA","119","Franklin","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",469.5544982949,"A","CEC Survey",2017,15,"I",559.636334347578,"TON",8,{"v":1.1918453265378002,"d":"1.19"},{"$f":"VLOOKUP(A6690,cordwood_density!A:D,4,FALSE)","v":1.3582},{"v":0.8775182790000001,"d":"0.88"}]
["13125","13","GA","125","Glascock","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",43.75671655515,"A","CEC Survey",2017,15,"I",27.4257709544914,"TON",8,{"v":0.6267785408423999,"d":"0.63"},{"$f":"VLOOKUP(A6729,cordwood_density!A:D,4,FALSE)","v":1.3257},{"v":0.47279063199999993,"d":"0.47"}]
["13127","13","GA","127","Glynn","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",713.2401181880001,"A","CEC Survey",2017,15,"I",558.3825517403046,"TON",8,{"v":0.7828815815337,"d":"0.78"},{"$f":"VLOOKUP(A6749,cordwood_density!A:D,4,FALSE)","v":1.2351},{"v":0.633860887,"d":"0.63"}]
["13131","13","GA","131","Grady","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.608655260467874,"A","CEC Survey",2017,15,"I",4.8309948329125625,"TON",8,{"v":1.8519100266418882,"d":"1.85"},{"$f":"VLOOKUP(A6768,cordwood_density!A:D,4,FALSE)","v":1.3453},{"v":1.3765777348114832,"d":"1.38"}]
["13133","13","GA","133","Greene","","2104008620","Hydronic heater: indoor","Hydronic heater",25.566424804511218,"A","CEC Survey",2017,15,"I",43.11818735647638,"TON",8,{"v":1.6865161118995464,"d":"1.69"},{"$f":"VLOOKUP(A6785,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":1.402858186574236,"d":"1.40"}]
["13137","13","GA","137","Habersham","","2104008610","Hydronic heater: outdoor","Hydronic heater",92.6851484212196,"A","CEC Survey",2017,15,"I",173.230932865592,"TON",8,{"v":1.869025791255377,"d":"1.87"},{"$f":"VLOOKUP(A6814,cordwood_density!A:D,4,FALSE)","v":1.2828},{"v":1.4569892354656822,"d":"1.46"}]
["13137","13","GA","137","Habersham","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",644.5284752761401,"A","CEC Survey",2017,15,"I",693.8787778966965,"TON",8,{"v":1.0765680718752,"d":"1.08"},{"$f":"VLOOKUP(A6824,cordwood_density!A:D,4,FALSE)","v":1.2828},{"v":0.839232984,"d":"0.84"}]
["13143","13","GA","143","Haralson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",315.4962091545,"A","CEC Survey",2017,15,"I",211.9185851685158,"TON",8,{"v":0.671699307375,"d":"0.67"},{"$f":"VLOOKUP(A6863,cordwood_density!A:D,4,FALSE)","v":1.2483},{"v":0.53809125,"d":"0.54"}]
["13143","13","GA","143","Haralson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",419.220834802,"A","CEC Survey",2017,15,"I",131.9083177744093,"TON",8,{"v":0.31465115,"d":"0.31"},{"$f":"VLOOKUP(A6867,cordwood_density!A:D,4,FALSE)","v":1.2483},{"v":0.2520637266682689,"d":"0.25"}]
["13149","13","GA","149","Heard","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",28.790726163396606,"A","CEC Survey",2017,15,"I",49.953574149877625,"TON",8,{"v":1.7350578052937973,"d":"1.74"},{"$f":"VLOOKUP(A6902,cordwood_density!A:D,4,FALSE)","v":1.1914},{"v":1.456318453327008,"d":"1.46"}]
["13151","13","GA","151","Henry","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1405.2801394651,"A","CEC Survey",2017,15,"I",811.2113596837253,"TON",8,{"v":0.57725953488,"d":"0.58"},{"$f":"VLOOKUP(A6923,cordwood_density!A:D,4,FALSE)","v":1.26},{"v":0.458142488,"d":"0.46"}]
["13153","13","GA","153","Houston","","2104009000","Wax Log; Total: All Combustor Types",null,792.8360641512759,"A","CEC Survey",2017,15,"I",185.62853122268575,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A6943,cordwood_density!A:D,4,FALSE)","v":1.3353},{"v":0.1753405976185127,"d":"0.18"}]
["13155","13","GA","155","Irwin","","2104009000","Wax Log; Total: All Combustor Types",null,47.728156543019736,"A","CEC Survey",2017,15,"I",11.174703066177258,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A6958,cordwood_density!A:D,4,FALSE)","v":1.3262},{"v":0.17654373397677572,"d":"0.18"}]
["13159","13","GA","159","Jasper","","2104008610","Hydronic heater: outdoor","Hydronic heater",29.420184506396645,"A","CEC Survey",2017,15,"I",52.7939722497365,"TON",8,{"$f":"P6979/J6979","v":{"v":1.7944813445428203,"d":"1.79"}},{"$f":"VLOOKUP(A6979,cordwood_density!A:D,4,FALSE)","v":1.2802},{"$f":"S6979/T6979","v":{"v":1.4017195317472428,"d":"1.40"}}]
["13163","13","GA","163","Jefferson","","2104009000","Wax Log; Total: All Combustor Types",null,83.26214970806062,"A","CEC Survey",2017,15,"I",19.49435861409256,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A7018,cordwood_density!A:D,4,FALSE)","v":1.3577},{"v":0.1724477425057082,"d":"0.17"}]
["13167","13","GA","167","Johnson","","2104008620","Hydronic heater: indoor","Hydronic heater",9.649718051253698,"A","CEC Survey",2017,15,"I",17.17840082163431,"TON",8,{"v":1.7801971757508996,"d":"1.78"},{"$f":"VLOOKUP(A7040,cordwood_density!A:D,4,FALSE)","v":1.27},{"v":1.4017300596463778,"d":"1.40"}]
["13169","13","GA","169","Jones","","2104008100","Fireplace: general","Fireplace: general",1382.329049024,"A","CEC Survey",2017,15,"I",400.8758438934416,"TON",8,{"v":0.290000303601,"d":"0.29"},{"$f":"VLOOKUP(A7057,cordwood_density!A:D,4,FALSE)","v":1.2421},{"v":0.23347581,"d":"0.23"}]
["13171","13","GA","171","Lamar","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",228.31750802304498,"A","CEC Survey",2017,15,"I",154.35604829550692,"TON",8,{"v":0.6760587465764,"d":"0.68"},{"$f":"VLOOKUP(A7074,cordwood_density!A:D,4,FALSE)","v":1.4036},{"v":0.481660549,"d":"0.48"}]
["13175","13","GA","175","Laurens","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",472.7362353554401,"A","CEC Survey",2017,15,"I",264.8189005169924,"TON",8,{"v":0.560183207276,"d":"0.56"},{"$f":"VLOOKUP(A7105,cordwood_density!A:D,4,FALSE)","v":1.2418},{"v":0.45110582,"d":"0.45"}]
["13177","13","GA","177","Lee","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.528067868985498,"A","CEC Survey",2017,15,"I",4.572535859410123,"TON",8,{"v":1.8087077152897246,"d":"1.81"},{"$f":"VLOOKUP(A7113,cordwood_density!A:D,4,FALSE)","v":1.3399},{"v":1.3498826145904355,"d":"1.35"}]
["13181","13","GA","181","Lincoln","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",135.726364458,"A","CEC Survey",2017,15,"I",46.787691300481455,"TON",8,{"v":0.344720729,"d":"0.34"},{"$f":"VLOOKUP(A7152,cordwood_density!A:D,4,FALSE)","v":1.2661},{"v":0.27226974883500515,"d":"0.27"}]
["13183","13","GA","183","Long","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.690632976266764,"A","CEC Survey",2017,15,"I",3.180105822149474,"TON",8,{"v":1.881014901987625,"d":"1.88"},{"$f":"VLOOKUP(A7158,cordwood_density!A:D,4,FALSE)","v":1.3011},{"v":1.445711245859369,"d":"1.45"}]
["13187","13","GA","187","Lumpkin","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.655235564930427,"A","CEC Survey",2017,15,"I",5.523212593023413,"TON",8,{"v":2.0801215025786735,"d":"2.08"},{"$f":"VLOOKUP(A7191,cordwood_density!A:D,4,FALSE)","v":1.3697},{"v":1.5186694185432383,"d":"1.52"}]
["13189","13","GA","189","McDuffie","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",216.66090272048,"A","CEC Survey",2017,15,"I",124.26485635347528,"TON",8,{"v":0.5735453641757999,"d":"0.57"},{"$f":"VLOOKUP(A7208,cordwood_density!A:D,4,FALSE)","v":1.1598},{"v":0.49452092099999995,"d":"0.49"}]
["13193","13","GA","193","Macon","","2104008610","Hydronic heater: outdoor","Hydronic heater",18.258398151744494,"A","CEC Survey",2017,15,"I",35.881166793385844,"TON",8,{"v":1.9651870057372798,"d":"1.97"},{"$f":"VLOOKUP(A7234,cordwood_density!A:D,4,FALSE)","v":1.3834},{"v":1.4205486524051467,"d":"1.42"}]
["13195","13","GA","195","Madison","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",68.49344347935724,"A","CEC Survey",2017,15,"I",116.01092732573125,"TON",8,{"v":1.6937522985056952,"d":"1.69"},{"$f":"VLOOKUP(A7247,cordwood_density!A:D,4,FALSE)","v":1.1474},{"v":1.476165503316799,"d":"1.48"}]
["13197","13","GA","197","Marion","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",95.54074330323003,"A","CEC Survey",2017,15,"I",51.761362551819666,"TON",8,{"v":0.5417726591004,"d":"0.54"},{"$f":"VLOOKUP(A7268,cordwood_density!A:D,4,FALSE)","v":1.2831},{"v":0.422237284,"d":"0.42"}]
["13205","13","GA","205","Mitchell","","2104008620","Hydronic heater: indoor","Hydronic heater",15.604214598266474,"A","CEC Survey",2017,15,"I",25.03591704471889,"TON",8,{"v":1.604433013084825,"d":"1.60"},{"$f":"VLOOKUP(A7310,cordwood_density!A:D,4,FALSE)","v":1.1711},{"v":1.3700222125222654,"d":"1.37"}]
["13207","13","GA","207","Monroe","","2104008620","Hydronic heater: indoor","Hydronic heater",33.36231983857822,"A","CEC Survey",2017,15,"I",63.65938400762962,"TON",8,{"v":1.9081222263812019,"d":"1.91"},{"$f":"VLOOKUP(A7325,cordwood_density!A:D,4,FALSE)","v":1.3803},{"v":1.3823967444622196,"d":"1.38"}]
["13209","13","GA","209","Montgomery","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,452.1071025419311,"A","CEC Survey",2017,15,"I",99.21925063277865,"TON",8,{"v":0.21945961493399999,"d":"0.22"},{"$f":"VLOOKUP(A7346,cordwood_density!A:D,4,FALSE)","v":1.2845},{"v":0.170852172,"d":"0.17"}]
["13211","13","GA","211","Morgan","","2104009000","Wax Log; Total: All Combustor Types",null,96.20318762486248,"A","CEC Survey",2017,15,"I",33.03894047202199,"TON",8,{"$f":"P7363/J7363","v":{"v":0.34342875,"d":"0.34"}},{"$f":"VLOOKUP(A7363,cordwood_density!A:D,4,FALSE)","v":1.1919},{"$f":"S7363/T7363","v":{"v":0.2881355398942865,"d":"0.29"}}]
["13215","13","GA","215","Muscogee","","2104008620","Hydronic heater: indoor","Hydronic heater",83.43957124250655,"A","CEC Survey",2017,15,"I",117.85101009579914,"TON",8,{"v":1.4124115014119631,"d":"1.41"},{"$f":"VLOOKUP(A7385,cordwood_density!A:D,4,FALSE)","v":1.3001},{"v":1.0863868174847804,"d":"1.09"}]
["13217","13","GA","217","Newton","","2104008100","Fireplace: general","Fireplace: general",4819.979312373,"A","CEC Survey",2017,15,"I",1236.8218088136716,"TON",8,{"v":0.2566031363742,"d":"0.26"},{"$f":"VLOOKUP(A7402,cordwood_density!A:D,4,FALSE)","v":1.2738},{"v":0.201446959,"d":"0.20"}]
["13221","13","GA","221","Oglethorpe","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",246.81577356072003,"A","CEC Survey",2017,15,"I",291.4781607805425,"TON",8,{"v":1.1809543473478,"d":"1.18"},{"$f":"VLOOKUP(A7441,cordwood_density!A:D,4,FALSE)","v":1.2638},{"v":0.9344471809999999,"d":"0.93"}]
["13223","13","GA","223","Paulding","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1548.60400335861,"A","CEC Survey",2017,15,"I",1152.6177097512448,"TON",8,{"v":0.7442946726544999,"d":"0.74"},{"$f":"VLOOKUP(A7449,cordwood_density!A:D,4,FALSE)","v":1.3795},{"v":0.5395394509999999,"d":"0.54"}]
["13227","13","GA","227","Pickens","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",320.53317300984,"A","CEC Survey",2017,15,"I",219.14898418333408,"TON",8,{"v":0.6837014157551999,"d":"0.68"},{"$f":"VLOOKUP(A7480,cordwood_density!A:D,4,FALSE)","v":1.1532},{"v":0.592873236,"d":"0.59"}]
["13229","13","GA","229","Pierce","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",236.12770215,"A","CEC Survey",2017,15,"I",52.51021960848289,"TON",8,{"v":0.222380598,"d":"0.22"},{"$f":"VLOOKUP(A7497,cordwood_density!A:D,4,FALSE)","v":1.2521},{"v":0.17760610015174508,"d":"0.18"}]
["13233","13","GA","233","Polk","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",335.115126423,"A","CEC Survey",2017,15,"I",221.10563121615715,"TON",8,{"v":0.6597900655104,"d":"0.66"},{"$f":"VLOOKUP(A7525,cordwood_density!A:D,4,FALSE)","v":1.3376},{"v":0.49326410400000004,"d":"0.49"}]
["13235","13","GA","235","Pulaski","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.4032593772523959,"A","CEC Survey",2017,15,"I",0.745832197228408,"TON",8,{"v":1.8495098670987613,"d":"1.85"},{"$f":"VLOOKUP(A7536,cordwood_density!A:D,4,FALSE)","v":1.3289},{"v":1.3917600023318244,"d":"1.39"}]
["13237","13","GA","237","Putnam","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",297.551878772,"A","CEC Survey",2017,15,"I",89.44366806946904,"TON",8,{"v":0.300598566,"d":"0.30"},{"$f":"VLOOKUP(A7557,cordwood_density!A:D,4,FALSE)","v":1.2806},{"v":0.23473259878182104,"d":"0.23"}]
["13243","13","GA","243","Randolph","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,430.62806716800003,"A","CEC Survey",2017,15,"I",93.49331612723688,"TON",8,{"v":0.21710920224519997,"d":"0.22"},{"$f":"VLOOKUP(A7601,cordwood_density!A:D,4,FALSE)","v":1.2788},{"v":0.169775729,"d":"0.17"}]
["13245","13","GA","245","Richmond","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1664.3871985359901,"A","CEC Survey",2017,15,"I",858.6177580190797,"TON",8,{"v":0.5158762088379,"d":"0.52"},{"$f":"VLOOKUP(A7614,cordwood_density!A:D,4,FALSE)","v":1.1827},{"v":0.4361851769999999,"d":"0.44"}]
["13247","13","GA","247","Rockdale","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",759.13107413118,"A","CEC Survey",2017,15,"I",551.1517816393571,"TON",8,{"v":0.7260297996234001,"d":"0.73"},{"$f":"VLOOKUP(A7635,cordwood_density!A:D,4,FALSE)","v":1.1838},{"v":0.6133044430000001,"d":"0.61"}]
["13251","13","GA","251","Screven","","2104008610","Hydronic heater: outdoor","Hydronic heater",22.965091397501343,"A","CEC Survey",2017,15,"I",40.33528551625578,"TON",8,{"v":1.756373829221701,"d":"1.76"},{"$f":"VLOOKUP(A7654,cordwood_density!A:D,4,FALSE)","v":1.2488},{"v":1.4064492546618363,"d":"1.41"}]
["13253","13","GA","253","Seminole","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",109.51405607316998,"A","CEC Survey",2017,15,"I",48.33490218239222,"TON",8,{"v":0.44135797646009994,"d":"0.44"},{"$f":"VLOOKUP(A7674,cordwood_density!A:D,4,FALSE)","v":1.3811},{"v":0.31956989099999994,"d":"0.32"}]
["13255","13","GA","255","Spalding","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3521.6194260750003,"A","CEC Survey",2017,15,"I",702.2398471317354,"TON",8,{"v":0.199408215985,"d":"0.20"},{"$f":"VLOOKUP(A7691,cordwood_density!A:D,4,FALSE)","v":1.1605},{"v":0.17182957,"d":"0.17"}]
["13261","13","GA","261","Sumter","","2104008620","Hydronic heater: indoor","Hydronic heater",20.44403906037151,"A","CEC Survey",2017,15,"I",33.44535021092616,"TON",8,{"v":1.635946307486579,"d":"1.64"},{"$f":"VLOOKUP(A7730,cordwood_density!A:D,4,FALSE)","v":1.236},{"v":1.3235811549244167,"d":"1.32"}]
["13263","13","GA","263","Talbot","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",104.91931180499999,"A","CEC Survey",2017,15,"I",38.29902709384996,"TON",8,{"v":0.365033152,"d":"0.37"},{"$f":"VLOOKUP(A7752,cordwood_density!A:D,4,FALSE)","v":1.2425},{"v":0.2937892571428572,"d":"0.29"}]
["13265","13","GA","265","Taliaferro","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",30.6680820638,"A","CEC Survey",2017,15,"I",36.84247227613613,"TON",8,{"v":1.201329519058,"d":"1.20"},{"$f":"VLOOKUP(A7769,cordwood_density!A:D,4,FALSE)","v":1.2724},{"v":0.944144545,"d":"0.94"}]
["13267","13","GA","267","Tattnall","","2104009000","Wax Log; Total: All Combustor Types",null,115.53574817463816,"A","CEC Survey",2017,15,"I",27.050650452348833,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A7783,cordwood_density!A:D,4,FALSE)","v":1.1826},{"v":0.19798097412480972,"d":"0.20"}]
["13271","13","GA","271","Telfair","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",161.94013070802998,"A","CEC Survey",2017,15,"I",96.42073393414393,"TON",8,{"v":0.595409757375,"d":"0.60"},{"$f":"VLOOKUP(A7808,cordwood_density!A:D,4,FALSE)","v":1.275},{"v":0.466988045,"d":"0.47"}]
["13273","13","GA","273","Terrell","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",81.6316792424,"A","CEC Survey",2017,15,"I",39.85875242645301,"TON",8,{"v":0.488275542,"d":"0.49"},{"$f":"VLOOKUP(A7825,cordwood_density!A:D,4,FALSE)","v":1.2},{"v":0.406896285,"d":"0.41"}]
["13279","13","GA","279","Toombs","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",284.8066315605,"A","CEC Survey",2017,15,"I",144.11473318810818,"TON",8,{"v":0.506009050416,"d":"0.51"},{"$f":"VLOOKUP(A7868,cordwood_density!A:D,4,FALSE)","v":1.2148},{"v":0.4165369199999999,"d":"0.42"}]
["13279","13","GA","279","Toombs","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",376.6797385155,"A","CEC Survey",2017,15,"I",190.60335679717534,"TON",8,{"v":0.506009050416,"d":"0.51"},{"$f":"VLOOKUP(A7869,cordwood_density!A:D,4,FALSE)","v":1.2148},{"v":0.4165369199999999,"d":"0.42"}]
["13283","13","GA","283","Treutlen","","2104009000","Wax Log; Total: All Combustor Types",null,37.81770574112879,"A","CEC Survey",2017,15,"I",8.854346425893688,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A7903,cordwood_density!A:D,4,FALSE)","v":1.3232},{"v":0.1769439993954051,"d":"0.18"}]
["13287","13","GA","287","Turner","","2104008610","Hydronic heater: outdoor","Hydronic heater",8.811911740989745,"A","CEC Survey",2017,15,"I",15.704434266274657,"TON",8,{"v":1.7821824284988528,"d":"1.78"},{"$f":"VLOOKUP(A7924,cordwood_density!A:D,4,FALSE)","v":1.3223},{"v":1.3477897818186892,"d":"1.35"}]
["13289","13","GA","289","Twiggs","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",85.91701436640001,"A","CEC Survey",2017,15,"I",58.893098246908394,"TON",8,{"v":0.6854649068199,"d":"0.69"},{"$f":"VLOOKUP(A7945,cordwood_density!A:D,4,FALSE)","v":1.3579},{"v":0.504797781,"d":"0.50"}]
["13291","13","GA","291","Union","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",450.5054509643999,"A","CEC Survey",2017,15,"I",389.93043058323605,"TON",8,{"v":0.8655398724887999,"d":"0.87"},{"$f":"VLOOKUP(A7959,cordwood_density!A:D,4,FALSE)","v":1.3441},{"v":0.643954968,"d":"0.64"}]
["13297","13","GA","297","Walton","","2104008100","Fireplace: general","Fireplace: general",3696.4829256320004,"A","CEC Survey",2017,15,"I",878.7652781235984,"TON",8,{"v":0.23773010610439999,"d":"0.24"},{"$f":"VLOOKUP(A8002,cordwood_density!A:D,4,FALSE)","v":1.1206},{"v":0.21214537399999997,"d":"0.21"}]
["13299","13","GA","299","Ware","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1904.8488065360002,"A","CEC Survey",2017,15,"I",409.4187122309377,"TON",8,{"v":0.2149350178482,"d":"0.21"},{"$f":"VLOOKUP(A8021,cordwood_density!A:D,4,FALSE)","v":1.2714},{"v":0.16905381299999997,"d":"0.17"}]
["13301","13","GA","301","Warren","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",79.09355578320002,"A","CEC Survey",2017,15,"I",87.92578965515314,"TON",8,{"v":1.1116681856630999,"d":"1.11"},{"$f":"VLOOKUP(A8041,cordwood_density!A:D,4,FALSE)","v":1.2123},{"v":0.916990997,"d":"0.92"}]
["13305","13","GA","305","Wayne","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.925677765566359,"A","CEC Survey",2017,15,"I",5.177848987558669,"TON",8,{"v":1.769794694582959,"d":"1.77"},{"$f":"VLOOKUP(A8058,cordwood_density!A:D,4,FALSE)","v":1.2837},{"v":1.3786668961462638,"d":"1.38"}]
["13307","13","GA","307","Webster","","2104008610","Hydronic heater: outdoor","Hydronic heater",4.657191319025087,"A","CEC Survey",2017,15,"I",8.898826487214707,"TON",8,{"v":1.9107710801706,"d":"1.91"},{"$f":"VLOOKUP(A8074,cordwood_density!A:D,4,FALSE)","v":1.3181},{"v":1.4496404522954252,"d":"1.45"}]
["13309","13","GA","309","Wheeler","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",70.805646,"A","CEC Survey",2017,15,"I",22.42504094739606,"TON",8,{"v":0.31671261,"d":"0.32"},{"$f":"VLOOKUP(A8097,cordwood_density!A:D,4,FALSE)","v":1.3081},{"v":0.24211651249904442,"d":"0.24"}]
["13315","13","GA","315","Wilcox","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.35342116593421624,"A","CEC Survey",2017,15,"I",0.6680240176193211,"TON",8,{"v":1.8901641497715593,"d":"1.89"},{"$f":"VLOOKUP(A8136,cordwood_density!A:D,4,FALSE)","v":1.346},{"v":1.404282429250787,"d":"1.40"}]
["13315","13","GA","315","Wilcox","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",111.36147668159998,"A","CEC Survey",2017,15,"I",62.467053994772144,"TON",8,{"v":0.5609395264520001,"d":"0.56"},{"$f":"VLOOKUP(A8139,cordwood_density!A:D,4,FALSE)","v":1.346},{"v":0.416745562,"d":"0.42"}]
["13319","13","GA","319","Wilkinson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",194.33120790095998,"A","CEC Survey",2017,15,"I",233.24521864865602,"TON",8,{"v":1.2002458131559002,"d":"1.20"},{"$f":"VLOOKUP(A8175,cordwood_density!A:D,4,FALSE)","v":1.3097},{"v":0.916428047,"d":"0.92"}]
["15001","15","HI","001","Hawaii","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",106.93732644317414,"A","CEC Survey",2017,15,"I",67.11265174649955,"TON",8,{"v":0.6275886444773128,"d":"0.63"},{"$f":"VLOOKUP(A8192,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.6107324294251778,"d":"0.61"}]
["15003","15","HI","003","Honolulu","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",3671.64766375932,"A","CEC Survey",2017,15,"I",670.7651729167725,"TON",8,{"v":0.18268778334520003,"d":"0.18"},{"$f":"VLOOKUP(A8215,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.177781027,"d":"0.18"}]
["15005","15","HI","005","Kalawao","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,9.323268849000002,"A","CEC Survey",2017,15,"I",0.8241598080805412,"TON",8,{"v":0.08839815964,"d":"0.09"},{"$f":"VLOOKUP(A8231,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.0860239,"d":"0.09"}]
["16001","16","ID","001","Ada","","2104008620","Hydronic heater: indoor","Hydronic heater",295.20252456035047,"A","CEC Survey",2017,15,"I",597.0911208401798,"TON",8,{"v":2.022649100746806,"d":"2.02"},{"$f":"VLOOKUP(A8270,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9888388404590032,"d":"1.99"}]
["16003","16","ID","003","Adams","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,289.233680568,"A","CEC Survey",2017,15,"I",71.13863917776692,"TON",8,{"v":0.2459555852488,"d":"0.25"},{"$f":"VLOOKUP(A8291,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.239349538,"d":"0.24"}]
["16007","16","ID","007","Bear Lake","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",49.603734317690424,"A","CEC Survey",2017,15,"I",124.75113715884828,"TON",8,{"v":2.5149545467660017,"d":"2.51"},{"$f":"VLOOKUP(A8312,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.4474061373744664,"d":"2.45"}]
["16009","16","ID","009","Benewah","","2104008620","Hydronic heater: indoor","Hydronic heater",42.8775422104934,"A","CEC Survey",2017,15,"I",111.2682919821212,"TON",8,{"v":2.5950249535266168,"d":"2.60"},{"$f":"VLOOKUP(A8330,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.5516469552867425,"d":"2.55"}]
["16011","16","ID","011","Bingham","","2104008100","Fireplace: general","Fireplace: general",813.2697650279999,"A","CEC Survey",2017,15,"I",284.15259885343823,"TON",8,{"v":0.34939525735800003,"d":"0.35"},{"$f":"VLOOKUP(A8347,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.340010955,"d":"0.34"}]
["16013","16","ID","013","Blaine","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",83.48903319961175,"A","CEC Survey",2017,15,"I",29.682118913905292,"TON",8,{"v":0.35552117178,"d":"0.36"},{"$f":"VLOOKUP(A8365,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.34957834,"d":"0.35"}]
["16015","16","ID","015","Boise","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",238.61549158832003,"A","CEC Survey",2017,15,"I",349.7171579739849,"TON",8,{"v":1.4656096117068,"d":"1.47"},{"$f":"VLOOKUP(A8386,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.4262452429999999,"d":"1.43"}]
["16021","16","ID","021","Boundary","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",101.83612173280001,"A","CEC Survey",2017,15,"I",68.50668364533995,"TON",8,{"v":0.6727149706769999,"d":"0.67"},{"$f":"VLOOKUP(A8425,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.661469981,"d":"0.66"}]
["16021","16","ID","021","Boundary","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",367.1579636153,"A","CEC Survey",2017,15,"I",523.0549853387099,"TON",8,{"v":1.4246047673549997,"d":"1.42"},{"$f":"VLOOKUP(A8430,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.400791315,"d":"1.40"}]
["16027","16","ID","027","Canyon","","2104008610","Hydronic heater: outdoor","Hydronic heater",282.63748704387825,"A","CEC Survey",2017,15,"I",598.1816630923005,"TON",8,{"v":2.11642719212061,"d":"2.12"},{"$f":"VLOOKUP(A8464,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.0595827093427497,"d":"2.06"}]
["16029","16","ID","029","Caribou","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9433506752762237,"A","CEC Survey",2017,15,"I",2.2874481295824745,"TON",8,{"v":2.424812097487166,"d":"2.42"},{"$f":"VLOOKUP(A8481,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.384279348561619,"d":"2.38"}]
["16031","16","ID","031","Cassia","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",367.85444397156004,"A","CEC Survey",2017,15,"I",445.46284890092676,"TON",8,{"v":1.2109758525449996,"d":"1.21"},{"$f":"VLOOKUP(A8506,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.1907333849999997,"d":"1.19"}]
["16033","16","ID","033","Clark","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",28.35604781348,"A","CEC Survey",2017,15,"I",38.975399443407866,"TON",8,{"v":1.3745004134489998,"d":"1.37"},{"$f":"VLOOKUP(A8520,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.351524497,"d":"1.35"}]
["16039","16","ID","039","Elmore","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",184.34440507626,"A","CEC Survey",2017,15,"I",64.3788257987999,"TON",8,{"v":0.34923124340100004,"d":"0.35"},{"$f":"VLOOKUP(A8559,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.3433935530000001,"d":"0.34"}]
["16043","16","ID","043","Fremont","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",79.58849339811506,"A","CEC Survey",2017,15,"I",200.14361578547351,"TON",8,{"v":2.514730550110069,"d":"2.51"},{"$f":"VLOOKUP(A8582,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.4471881569774903,"d":"2.45"}]
["16045","16","ID","045","Gem","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.481263373113814,"A","CEC Survey",2017,15,"I",7.755244714873565,"TON",8,{"v":2.2277098523392933,"d":"2.23"},{"$f":"VLOOKUP(A8598,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.190471831208745,"d":"2.19"}]
["16047","16","ID","047","Gooding","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",139.0065927615,"A","CEC Survey",2017,15,"I",42.64328906161996,"TON",8,{"v":0.30677170207880006,"d":"0.31"},{"$f":"VLOOKUP(A8619,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.29853221300000005,"d":"0.30"}]
["16049","16","ID","049","Idaho","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",177.70683752640002,"A","CEC Survey",2017,15,"I",99.39661121556045,"TON",8,{"v":0.559329132177,"d":"0.56"},{"$f":"VLOOKUP(A8635,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.549979481,"d":"0.55"}]
["16051","16","ID","051","Jefferson","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",412.30559172110003,"A","CEC Survey",2017,15,"I",513.2998211698562,"TON",8,{"v":1.2449499387752,"d":"1.24"},{"$f":"VLOOKUP(A8654,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.211512202,"d":"1.21"}]
["16055","16","ID","055","Kootenai","","2104008620","Hydronic heater: indoor","Hydronic heater",380.13055367533883,"A","CEC Survey",2017,15,"I",920.2078127008434,"TON",8,{"v":2.4207678225380764,"d":"2.42"},{"$f":"VLOOKUP(A8675,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.3803026770285904,"d":"2.38"}]
["16059","16","ID","059","Lemhi","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",269.91315168139,"A","CEC Survey",2017,15,"I",375.6972917936108,"TON",8,{"v":1.3919191764212,"d":"1.39"},{"$f":"VLOOKUP(A8714,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.3545340369999999,"d":"1.35"}]
["16063","16","ID","063","Lincoln","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",19.491232203275015,"A","CEC Survey",2017,15,"I",46.68366811341923,"TON",8,{"v":2.3951111775055045,"d":"2.40"},{"$f":"VLOOKUP(A8732,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.3307816052019312,"d":"2.33"}]
["16065","16","ID","065","Madison","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",79.55517688846001,"A","CEC Survey",2017,15,"I",28.438982749463754,"TON",8,{"v":0.3574749483536,"d":"0.36"},{"$f":"VLOOKUP(A8753,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.347873636,"d":"0.35"}]
["16067","16","ID","067","Minidoka","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",124.98593888144,"A","CEC Survey",2017,15,"I",39.5083766304208,"TON",8,{"v":0.31610257108920004,"d":"0.32"},{"$f":"VLOOKUP(A8770,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.307612467,"d":"0.31"}]
["16071","16","ID","071","Oneida","","2104008100","Fireplace: general","Fireplace: general",65.112707148,"A","CEC Survey",2017,15,"I",25.083844636493964,"TON",8,{"v":0.3852373174944,"d":"0.39"},{"$f":"VLOOKUP(A8797,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.374890344,"d":"0.37"}]
["16073","16","ID","073","Owyhee","","2104008610","Hydronic heater: outdoor","Hydronic heater",54.44239629793528,"A","CEC Survey",2017,15,"I",132.59988212744977,"TON",8,{"v":2.435599663942026,"d":"2.44"},{"$f":"VLOOKUP(A8809,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.370182623532528,"d":"2.37"}]
["16077","16","ID","077","Power","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A8848,cordwood_density!A:D,4,FALSE)","v":1.017},{"$error":"#DIV/0!"}]
["16081","16","ID","081","Teton","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",86.81230207844,"A","CEC Survey",2017,15,"I",36.49849484183309,"TON",8,{"v":0.42042998478320004,"d":"0.42"},{"$f":"VLOOKUP(A8873,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.409137782,"d":"0.41"}]
["16083","16","ID","083","Twin Falls","","2104008100","Fireplace: general","Fireplace: general",1939.6325155680001,"A","CEC Survey",2017,15,"I",635.5160290877953,"TON",8,{"v":0.32764764664799995,"d":"0.33"},{"$f":"VLOOKUP(A8887,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.32217074399999995,"d":"0.32"}]
["16085","16","ID","085","Valley","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A8908,cordwood_density!A:D,4,FALSE)","v":1.017},{"$error":"#DIV/0!"}]
["16087","16","ID","087","Washington","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",131.68430581012,"A","CEC Survey",2017,15,"I",146.8332826561198,"TON",8,{"v":1.1150401086356,"d":"1.12"},{"$f":"VLOOKUP(A8926,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.085091581,"d":"1.09"}]
["17003","17","IL","003","Alexander","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.2845320952792214,"A","CEC Survey",2017,15,"I",4.062915941836897,"TON",8,{"v":3.162954010077679,"d":"3.16"},{"$f":"VLOOKUP(A8943,cordwood_density!A:D,4,FALSE)","v":1.4811},{"v":2.135543859346215,"d":"2.14"}]
["17005","17","IL","005","Bond","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",180.75855350196002,"A","CEC Survey",2017,15,"I",94.89870983288957,"TON",8,{"v":0.5250025959732,"d":"0.53"},{"$f":"VLOOKUP(A8964,cordwood_density!A:D,4,FALSE)","v":1.3694},{"v":0.383381478,"d":"0.38"}]
["17011","17","IL","011","Bureau","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",123.22819499274927,"A","CEC Survey",2017,15,"I",357.7933635484908,"TON",8,{"v":2.903502429533625,"d":"2.90"},{"$f":"VLOOKUP(A9002,cordwood_density!A:D,4,FALSE)","v":1.3092},{"v":2.2177684307467347,"d":"2.22"}]
["17013","17","IL","013","Calhoun","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.624326192115893,"A","CEC Survey",2017,15,"I",2.014681390807298,"TON",8,{"v":3.2269691969503578,"d":"3.23"},{"$f":"VLOOKUP(A9021,cordwood_density!A:D,4,FALSE)","v":1.4339},{"v":2.250484132052694,"d":"2.25"}]
["17015","17","IL","015","Carroll","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",304.067696457,"A","CEC Survey",2017,15,"I",155.88443747681129,"TON",8,{"v":0.512663592,"d":"0.51"},{"$f":"VLOOKUP(A9042,cordwood_density!A:D,4,FALSE)","v":1.3591},{"v":0.3772081465675815,"d":"0.38"}]
["17017","17","IL","017","Cass","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",84.487284252,"A","CEC Survey",2017,15,"I",46.482463919408836,"TON",8,{"v":0.5501711213816001,"d":"0.55"},{"$f":"VLOOKUP(A9055,cordwood_density!A:D,4,FALSE)","v":1.4114},{"v":0.38980524400000005,"d":"0.39"}]
["17021","17","IL","021","Christian","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.000155037820471,"A","CEC Survey",2017,15,"I",5.518543710198234,"TON",8,{"v":2.759057975931546,"d":"2.76"},{"$f":"VLOOKUP(A9081,cordwood_density!A:D,4,FALSE)","v":1.3381},{"v":2.061922110403965,"d":"2.06"}]
["17023","17","IL","023","Clark","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",45.65373545831999,"A","CEC Survey",2017,15,"I",24.384050120101975,"TON",8,{"v":0.5341085428237,"d":"0.53"},{"$f":"VLOOKUP(A9098,cordwood_density!A:D,4,FALSE)","v":1.3397},{"v":0.39867772100000004,"d":"0.40"}]
["17029","17","IL","029","Coles","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",80.76500295006564,"A","CEC Survey",2017,15,"I",227.94576354966952,"TON",8,{"v":2.8223333773738726,"d":"2.82"},{"$f":"VLOOKUP(A9137,cordwood_density!A:D,4,FALSE)","v":1.3611},{"v":2.0735679798500275,"d":"2.07"}]
["17029","17","IL","029","Coles","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.1828379175693415,"A","CEC Survey",2017,15,"I",6.160696312153231,"TON",8,{"v":2.8223333773738726,"d":"2.82"},{"$f":"VLOOKUP(A9141,cordwood_density!A:D,4,FALSE)","v":1.3611},{"v":2.0735679798500275,"d":"2.07"}]
["17033","17","IL","033","Crawford","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1210.69125702,"A","CEC Survey",2017,15,"I",410.25481088076026,"TON",8,{"v":0.33885997648200006,"d":"0.34"},{"$f":"VLOOKUP(A9176,cordwood_density!A:D,4,FALSE)","v":1.4004},{"v":0.24197370500000004,"d":"0.24"}]
["17035","17","IL","035","Cumberland","","2104009000","Wax Log; Total: All Combustor Types",null,68.77128390206484,"A","CEC Survey",2017,15,"I",38.367450838904745,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A9193,cordwood_density!A:D,4,FALSE)","v":1.3566},{"v":0.41124819068996016,"d":"0.41"}]
["17039","17","IL","039","Dewitt","","2104008100","Fireplace: general","Fireplace: general",609.2374235251233,"A","CEC Survey",2017,15,"I",248.38168938239522,"TON",8,{"v":0.40769276441560004,"d":"0.41"},{"$f":"VLOOKUP(A9217,cordwood_density!A:D,4,FALSE)","v":1.1867},{"v":0.34355166800000003,"d":"0.34"}]
["17041","17","IL","041","Douglas","","2104008100","Fireplace: general","Fireplace: general",541.9897914515026,"A","CEC Survey",2017,15,"I",262.83054298724187,"TON",8,{"v":0.48493633484010007,"d":"0.48"},{"$f":"VLOOKUP(A9232,cordwood_density!A:D,4,FALSE)","v":1.3277},{"v":0.365245413,"d":"0.37"}]
["17043","17","IL","043","Du Page","","2104009000","Wax Log; Total: All Combustor Types",null,11710.79953690818,"A","CEC Survey",2017,15,"I",9140.213458079426,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A9253,cordwood_density!A:D,4,FALSE)","v":1.3279},{"v":0.5877659462308907,"d":"0.59"}]
["17049","17","IL","049","Effingham","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",83.50718985,"A","CEC Survey",2017,15,"I",48.93954848717637,"TON",8,{"v":0.5860519145128,"d":"0.59"},{"$f":"VLOOKUP(A9293,cordwood_density!A:D,4,FALSE)","v":1.4486},{"v":0.404564348,"d":"0.40"}]
["17051","17","IL","051","Fayette","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",148.96400196825,"A","CEC Survey",2017,15,"I",87.4658621129636,"TON",8,{"v":0.5871610654741001,"d":"0.59"},{"$f":"VLOOKUP(A9310,cordwood_density!A:D,4,FALSE)","v":1.4677},{"v":0.40005523300000007,"d":"0.40"}]
["17053","17","IL","053","Ford","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",199.70278367046578,"A","CEC Survey",2017,15,"I",306.5461998956343,"TON",8,{"v":1.5350121528675,"d":"1.54"},{"$f":"VLOOKUP(A9331,cordwood_density!A:D,4,FALSE)","v":1.4389},{"v":1.066795575,"d":"1.07"}]
["17055","17","IL","055","Franklin","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",609.8893124555,"A","CEC Survey",2017,15,"I",945.0170283519046,"TON",8,{"v":1.5494894057859998,"d":"1.55"},{"$f":"VLOOKUP(A9346,cordwood_density!A:D,4,FALSE)","v":1.418},{"v":1.0927287769999998,"d":"1.09"}]
["17059","17","IL","059","Gallatin","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",40.968242784,"A","CEC Survey",2017,15,"I",22.752977215204346,"TON",8,{"v":0.555380843039,"d":"0.56"},{"$f":"VLOOKUP(A9370,cordwood_density!A:D,4,FALSE)","v":1.3714},{"v":0.40497363500000005,"d":"0.40"}]
["17061","17","IL","061","Greene","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",217.64353570699998,"A","CEC Survey",2017,15,"I",83.22634176908217,"TON",8,{"v":0.38239749,"d":"0.38"},{"$f":"VLOOKUP(A9387,cordwood_density!A:D,4,FALSE)","v":1.4117},{"v":0.27087730395976484,"d":"0.27"}]
["17067","17","IL","067","Hancock","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",70.0962407222558,"A","CEC Survey",2017,15,"I",211.61483168972808,"TON",8,{"v":3.0189184114482708,"d":"3.02"},{"$f":"VLOOKUP(A9422,cordwood_density!A:D,4,FALSE)","v":1.3747},{"v":2.196056166034968,"d":"2.20"}]
["17069","17","IL","069","Hardin","","2104009000","Wax Log; Total: All Combustor Types",null,23.292723163635504,"A","CEC Survey",2017,15,"I",12.99499384303585,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A9448,cordwood_density!A:D,4,FALSE)","v":1.4499},{"v":0.3847846716945996,"d":"0.38"}]
["17071","17","IL","071","Henderson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",219.72843829862,"A","CEC Survey",2017,15,"I",370.69366638845764,"TON",8,{"v":1.6870536615960001,"d":"1.69"},{"$f":"VLOOKUP(A9465,cordwood_density!A:D,4,FALSE)","v":1.332},{"v":1.266556803,"d":"1.27"}]
["17077","17","IL","077","Jackson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.471948984592144,"A","CEC Survey",2017,15,"I",25.45185965007716,"TON",8,{"v":3.0042508160006896,"d":"3.00"},{"$f":"VLOOKUP(A9498,cordwood_density!A:D,4,FALSE)","v":1.4413},{"v":2.0844035356974184,"d":"2.08"}]
["17077","17","IL","077","Jackson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",643.90506567674,"A","CEC Survey",2017,15,"I",477.1794952583361,"TON",8,{"v":0.7410711930909001,"d":"0.74"},{"$f":"VLOOKUP(A9504,cordwood_density!A:D,4,FALSE)","v":1.4413},{"v":0.5141685930000001,"d":"0.51"}]
["17079","17","IL","079","Jasper","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,588.677070507,"A","CEC Survey",2017,15,"I",198.13166933113976,"TON",8,{"v":0.3365710663072,"d":"0.34"},{"$f":"VLOOKUP(A9521,cordwood_density!A:D,4,FALSE)","v":1.3918},{"v":0.24182430400000002,"d":"0.24"}]
["17085","17","IL","085","Jo Daviess","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",263.7319075257,"A","CEC Survey",2017,15,"I",136.9967375427196,"TON",8,{"v":0.5194545431684999,"d":"0.52"},{"$f":"VLOOKUP(A9564,cordwood_density!A:D,4,FALSE)","v":1.2945},{"v":0.4012781329999999,"d":"0.40"}]
["17087","17","IL","087","Johnson","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",94.68223609271999,"A","CEC Survey",2017,15,"I",181.6513277286925,"TON",8,{"v":1.9185365198896003,"d":"1.92"},{"$f":"VLOOKUP(A9584,cordwood_density!A:D,4,FALSE)","v":1.4456},{"v":1.3271558660000002,"d":"1.33"}]
["17089","17","IL","089","Kane","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1220.7780799956,"A","CEC Survey",2017,15,"I",1337.8013539024314,"TON",8,{"v":1.095859579906,"d":"1.10"},{"$f":"VLOOKUP(A9599,cordwood_density!A:D,4,FALSE)","v":1.3364},{"v":0.820008665,"d":"0.82"}]
["17093","17","IL","093","Kendall","","2104008620","Hydronic heater: indoor","Hydronic heater",109.96365100229589,"A","CEC Survey",2017,15,"I",329.8379859950459,"TON",8,{"v":2.9995183225424134,"d":"3.00"},{"$f":"VLOOKUP(A9620,cordwood_density!A:D,4,FALSE)","v":1.3956},{"v":2.149267929594736,"d":"2.15"}]
["17095","17","IL","095","Knox","","2104008100","Fireplace: general","Fireplace: general",2119.5017110119998,"A","CEC Survey",2017,15,"I",872.9890383123076,"TON",8,{"v":0.4118840922735,"d":"0.41"},{"$f":"VLOOKUP(A9637,cordwood_density!A:D,4,FALSE)","v":1.3365},{"v":0.308181139,"d":"0.31"}]
["17097","17","IL","097","Lake","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1639.0611040843198,"A","CEC Survey",2017,15,"I",1720.41134617423,"TON",8,{"v":1.0496322204750002,"d":"1.05"},{"$f":"VLOOKUP(A9659,cordwood_density!A:D,4,FALSE)","v":1.3873},{"v":0.7566007500000002,"d":"0.76"}]
["17103","17","IL","103","Lee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",63.26171302463999,"A","CEC Survey",2017,15,"I",28.29605597754385,"TON",8,{"v":0.4472856428425,"d":"0.45"},{"$f":"VLOOKUP(A9698,cordwood_density!A:D,4,FALSE)","v":1.3069},{"v":0.342249325,"d":"0.34"}]
["17105","17","IL","105","Livingston","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",66.02307480252,"A","CEC Survey",2017,15,"I",26.960733544601677,"TON",8,{"v":0.4083531950798,"d":"0.41"},{"$f":"VLOOKUP(A9713,cordwood_density!A:D,4,FALSE)","v":1.2574},{"v":0.324759977,"d":"0.32"}]
["17109","17","IL","109","McDonough","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",55.71690885587926,"A","CEC Survey",2017,15,"I",160.96731780593095,"TON",8,{"v":2.889020965292579,"d":"2.89"},{"$f":"VLOOKUP(A9737,cordwood_density!A:D,4,FALSE)","v":1.3255},{"v":2.179570701842761,"d":"2.18"}]
["17111","17","IL","111","McHenry","","2104008610","Hydronic heater: outdoor","Hydronic heater",512.170374895213,"A","CEC Survey",2017,15,"I",1495.5701831625556,"TON",8,{"v":2.920063823427,"d":"2.92"},{"$f":"VLOOKUP(A9754,cordwood_density!A:D,4,FALSE)","v":1.3986},{"v":2.0878477215980267,"d":"2.09"}]
["17111","17","IL","111","McHenry","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2680.4933242989996,"A","CEC Survey",2017,15,"I",3445.819691239873,"TON",8,{"v":1.2855169830132,"d":"1.29"},{"$f":"VLOOKUP(A9766,cordwood_density!A:D,4,FALSE)","v":1.3986},{"v":0.919145562,"d":"0.92"}]
["17115","17","IL","115","Macon","","2104009000","Wax Log; Total: All Combustor Types",null,710.8130601795381,"A","CEC Survey",2017,15,"I",554.7856129169924,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A9793,cordwood_density!A:D,4,FALSE)","v":1.1375},{"v":0.686148923076923,"d":"0.69"}]
["17121","17","IL","121","Marion","","2104008100","Fireplace: general","Fireplace: general",1391.4275187849998,"A","CEC Survey",2017,15,"I",651.0429447465706,"TON",8,{"v":0.4678956941394,"d":"0.47"},{"$f":"VLOOKUP(A9832,cordwood_density!A:D,4,FALSE)","v":1.4358},{"v":0.325878043,"d":"0.33"}]
["17123","17","IL","123","Marshall","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",83.26627016399999,"A","CEC Survey",2017,15,"I",141.1873891459174,"TON",8,{"v":1.6956132281155003,"d":"1.70"},{"$f":"VLOOKUP(A9854,cordwood_density!A:D,4,FALSE)","v":1.3681},{"v":1.2393927550000001,"d":"1.24"}]
["17125","17","IL","125","Mason","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",273.4534454632812,"A","CEC Survey",2017,15,"I",471.82447309247624,"TON",8,{"v":1.7254288834909997,"d":"1.73"},{"$f":"VLOOKUP(A9871,cordwood_density!A:D,4,FALSE)","v":1.4318},{"v":1.2050767449999997,"d":"1.21"}]
["17129","17","IL","129","Menard","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.878566938152428,"A","CEC Survey",2017,15,"I",10.456195155028244,"TON",8,{"v":2.6958913747687174,"d":"2.70"},{"$f":"VLOOKUP(A9888,cordwood_density!A:D,4,FALSE)","v":1.2526},{"v":2.1522364480031277,"d":"2.15"}]
["17131","17","IL","131","Mercer","","2104008100","Fireplace: general","Fireplace: general",568.6392919658972,"A","CEC Survey",2017,15,"I",272.84136981886087,"TON",8,{"v":0.4798144863954,"d":"0.48"},{"$f":"VLOOKUP(A9907,cordwood_density!A:D,4,FALSE)","v":1.3287},{"v":0.36111574199999996,"d":"0.36"}]
["17133","17","IL","133","Monroe","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",476.586071235,"A","CEC Survey",2017,15,"I",151.85277120023773,"TON",8,{"v":0.318626121,"d":"0.32"},{"$f":"VLOOKUP(A9927,cordwood_density!A:D,4,FALSE)","v":1.406},{"v":0.2266188627311522,"d":"0.23"}]
["17139","17","IL","139","Moultrie","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0790146309177906,"A","CEC Survey",2017,15,"I",2.8447212699745137,"TON",8,{"v":2.63640657731846,"d":"2.64"},{"$f":"VLOOKUP(A9966,cordwood_density!A:D,4,FALSE)","v":1.2542},{"v":2.102062332417844,"d":"2.10"}]
["17141","17","IL","141","Ogle","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",766.90508805,"A","CEC Survey",2017,15,"I",329.46701575323203,"TON",8,{"$f":"P9987/J9987","v":{"v":0.4296059850000001,"d":"0.43"}},{"$f":"VLOOKUP(A9987,cordwood_density!A:D,4,FALSE)","v":1.3684},{"$f":"S9987/T9987","v":{"v":0.31394766515638706,"d":"0.31"}}]
["17143","17","IL","143","Peoria","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",639.4068007487999,"A","CEC Survey",2017,15,"I",834.1243307865384,"TON",8,{"v":1.3045284000885002,"d":"1.30"},{"$f":"VLOOKUP(A10004,cordwood_density!A:D,4,FALSE)","v":1.3459},{"v":0.9692610150000001,"d":"0.97"}]
["17147","17","IL","147","Piatt","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.4727119265526665,"A","CEC Survey",2017,15,"I",4.100869873149707,"TON",8,{"v":2.784570287788087,"d":"2.78"},{"$f":"VLOOKUP(A10026,cordwood_density!A:D,4,FALSE)","v":1.3067},{"v":2.130994327533548,"d":"2.13"}]
["17149","17","IL","149","Pike","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",41.93583463736611,"A","CEC Survey",2017,15,"I",24.890573495552243,"TON",8,{"v":0.5935394802748001,"d":"0.59"},{"$f":"VLOOKUP(A10043,cordwood_density!A:D,4,FALSE)","v":1.3861},{"v":0.428208268,"d":"0.43"}]
["17151","17","IL","151","Pope","","2104008100","Fireplace: general","Fireplace: general",176.969818696,"A","CEC Survey",2017,15,"I",89.03705065084233,"TON",8,{"v":0.5031199743939999,"d":"0.50"},{"$f":"VLOOKUP(A10057,cordwood_density!A:D,4,FALSE)","v":1.4156},{"v":0.35541111499999994,"d":"0.36"}]
["17155","17","IL","155","Putnam","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",34.0910087896071,"A","CEC Survey",2017,15,"I",107.37073433547354,"TON",8,{"v":3.1495323297152273,"d":"3.15"},{"$f":"VLOOKUP(A10082,cordwood_density!A:D,4,FALSE)","v":1.3958},{"v":2.256435255563281,"d":"2.26"}]
["17159","17","IL","159","Richland","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,922.77835762,"A","CEC Survey",2017,15,"I",321.1354051610875,"TON",8,{"v":0.348009251094,"d":"0.35"},{"$f":"VLOOKUP(A10121,cordwood_density!A:D,4,FALSE)","v":1.4436},{"v":0.241070415,"d":"0.24"}]
["17163","17","IL","163","St Clair","","2104008620","Hydronic heater: indoor","Hydronic heater",179.35741484408837,"A","CEC Survey",2017,15,"I",483.1061630050997,"TON",8,{"v":2.69353883933404,"d":"2.69"},{"$f":"VLOOKUP(A10145,cordwood_density!A:D,4,FALSE)","v":1.3866},{"v":1.9425492855430835,"d":"1.94"}]
["17165","17","IL","165","Saline","","2104008620","Hydronic heater: indoor","Hydronic heater",31.488197939791476,"A","CEC Survey",2017,15,"I",87.1841084752722,"TON",8,{"v":2.7687868528385384,"d":"2.77"},{"$f":"VLOOKUP(A10160,cordwood_density!A:D,4,FALSE)","v":1.3402},{"v":2.0659504945818075,"d":"2.07"}]
["17167","17","IL","167","Sangamon","","2104008100","Fireplace: general","Fireplace: general",7726.743691344,"A","CEC Survey",2017,15,"I",2917.115081695813,"TON",8,{"v":0.37753485791999997,"d":"0.38"},{"$f":"VLOOKUP(A10177,cordwood_density!A:D,4,FALSE)","v":1.2696},{"v":0.29736519999999994,"d":"0.30"}]
["17169","17","IL","169","Schuyler","","2104009000","Wax Log; Total: All Combustor Types",null,45.81543894996074,"A","CEC Survey",2017,15,"I",35.75869353398624,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A10198,cordwood_density!A:D,4,FALSE)","v":1.42},{"v":0.5496439436619718,"d":"0.55"}]
["17171","17","IL","171","Scott","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",104.11229848914999,"A","CEC Survey",2017,15,"I",181.78881037152755,"TON",8,{"v":1.7460839210122,"d":"1.75"},{"$f":"VLOOKUP(A10216,cordwood_density!A:D,4,FALSE)","v":1.3909},{"v":1.255362658,"d":"1.26"}]
["17177","17","IL","177","Stephenson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",256.4548220598,"A","CEC Survey",2017,15,"I",113.06468144705964,"TON",8,{"v":0.44087563079900005,"d":"0.44"},{"$f":"VLOOKUP(A10255,cordwood_density!A:D,4,FALSE)","v":1.2757},{"v":0.34559507,"d":"0.35"}]
["17179","17","IL","179","Tazewell","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",507.0728342551199,"A","CEC Survey",2017,15,"I",653.8915138225304,"TON",8,{"v":1.2895415996463,"d":"1.29"},{"$f":"VLOOKUP(A10274,cordwood_density!A:D,4,FALSE)","v":1.3167},{"v":0.979373889,"d":"0.98"}]
["17183","17","IL","183","Vermilion","","2104008610","Hydronic heater: outdoor","Hydronic heater",169.29194452880662,"A","CEC Survey",2017,15,"I",489.187025056857,"TON",8,{"v":2.8896060377735058,"d":"2.89"},{"$f":"VLOOKUP(A10294,cordwood_density!A:D,4,FALSE)","v":1.3397},{"v":2.1569053054963843,"d":"2.16"}]
["17185","17","IL","185","Wabash","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",83.71421675574999,"A","CEC Survey",2017,15,"I",43.326275444166605,"TON",8,{"v":0.5175497916988001,"d":"0.52"},{"$f":"VLOOKUP(A10315,cordwood_density!A:D,4,FALSE)","v":1.4252},{"v":0.36314186900000006,"d":"0.36"}]
["17187","17","IL","187","Warren","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",257.44861908015105,"A","CEC Survey",2017,15,"I",89.55111920261233,"TON",8,{"v":0.347840744,"d":"0.35"},{"$f":"VLOOKUP(A10332,cordwood_density!A:D,4,FALSE)","v":1.3975},{"v":0.24890214239713773,"d":"0.25"}]
["17189","17","IL","189","Washington","","2104009000","Wax Log; Total: All Combustor Types",null,94.59861468267997,"A","CEC Survey",2017,15,"I",52.776500485797115,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A10348,cordwood_density!A:D,4,FALSE)","v":1.427},{"v":0.39095956236159773,"d":"0.39"}]
["17193","17","IL","193","White","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9065585653532879,"A","CEC Survey",2017,15,"I",2.681306679070224,"TON",8,{"$f":"P10371/J10371","v":{"v":2.9576761850187943,"d":"2.96"}},{"$f":"VLOOKUP(A10371,cordwood_density!A:D,4,FALSE)","v":1.4473},{"$f":"S10371/T10371","v":{"v":2.043581969887925,"d":"2.04"}}]
["17197","17","IL","197","Will","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",7407.179828323081,"A","CEC Survey",2017,15,"I",8232.260635544784,"TON",8,{"v":1.111389331209,"d":"1.11"},{"$f":"VLOOKUP(A10410,cordwood_density!A:D,4,FALSE)","v":1.3215},{"v":0.841005926,"d":"0.84"}]
["17199","17","IL","199","Williamson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.648535864045893,"A","CEC Survey",2017,15,"I",33.15677021443324,"TON",8,{"v":2.8464324273382866,"d":"2.85"},{"$f":"VLOOKUP(A10413,cordwood_density!A:D,4,FALSE)","v":1.3582},{"v":2.095738792032312,"d":"2.10"}]
["17203","17","IL","203","Woodford","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",333.17809386615005,"A","CEC Survey",2017,15,"I",168.12193137728744,"TON",8,{"v":0.5046007960079999,"d":"0.50"},{"$f":"VLOOKUP(A10449,cordwood_density!A:D,4,FALSE)","v":1.4022},{"v":0.35986363999999993,"d":"0.36"}]
["18001","18","IN","001","Adams","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1752.790060602,"A","CEC Survey",2017,15,"I",596.8214964707367,"TON",8,{"v":0.34049799224999994,"d":"0.34"},{"$f":"VLOOKUP(A10466,cordwood_density!A:D,4,FALSE)","v":1.3635},{"v":0.24972349999999996,"d":"0.25"}]
["18005","18","IN","005","Bartholomew","","2104008610","Hydronic heater: outdoor","Hydronic heater",166.721980687254,"A","CEC Survey",2017,15,"I",505.4737600552621,"TON",8,{"v":3.0318363419845453,"d":"3.03"},{"$f":"VLOOKUP(A10489,cordwood_density!A:D,4,FALSE)","v":1.3541},{"v":2.239004757392028,"d":"2.24"}]
["18007","18","IN","007","Benton","","2104008620","Hydronic heater: indoor","Hydronic heater",24.76441142325737,"A","CEC Survey",2017,15,"I",71.45849106958121,"TON",8,{"v":2.885531573848403,"d":"2.89"},{"$f":"VLOOKUP(A10505,cordwood_density!A:D,4,FALSE)","v":1.26},{"v":2.2901044236892085,"d":"2.29"}]
["18011","18","IN","011","Boone","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",268.53346273824,"A","CEC Survey",2017,15,"I",369.85767008265407,"TON",8,{"v":1.3773243241688,"d":"1.38"},{"$f":"VLOOKUP(A10544,cordwood_density!A:D,4,FALSE)","v":1.2964},{"v":1.062422342,"d":"1.06"}]
["18015","18","IN","015","Carroll","","2104008620","Hydronic heater: indoor","Hydronic heater",54.23973133142427,"A","CEC Survey",2017,15,"I",159.75397248811066,"TON",8,{"v":2.945331191114433,"d":"2.95"},{"$f":"VLOOKUP(A10565,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":2.3229995986390355,"d":"2.32"}]
["18017","18","IN","017","Cass","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",77.27336043839999,"A","CEC Survey",2017,15,"I",38.752340941007446,"TON",8,{"v":0.5014967735472,"d":"0.50"},{"$f":"VLOOKUP(A10583,cordwood_density!A:D,4,FALSE)","v":1.3241},{"v":0.378745392,"d":"0.38"}]
["18019","18","IN","019","Clark","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",429.06742929552,"A","CEC Survey",2017,15,"I",571.5653231117816,"TON",8,{"v":1.3321107222009998,"d":"1.33"},{"$f":"VLOOKUP(A10604,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.0242278349999998,"d":"1.02"}]
["18021","18","IN","021","Clay","","2104009000","Wax Log; Total: All Combustor Types",null,171.32664145153387,"A","CEC Survey",2017,15,"I",95.58301256447857,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A10618,cordwood_density!A:D,4,FALSE)","v":1.3364},{"v":0.4174643037189464,"d":"0.42"}]
["18025","18","IN","025","Crawford","","2104008610","Hydronic heater: outdoor","Hydronic heater",49.435774983385436,"A","CEC Survey",2017,15,"I",156.41172549609595,"TON",8,{"v":3.1639379689842713,"d":"3.16"},{"$f":"VLOOKUP(A10639,cordwood_density!A:D,4,FALSE)","v":1.33},{"v":2.378900728559602,"d":"2.38"}]
["18027","18","IN","027","Daviess","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",208.98581040189995,"A","CEC Survey",2017,15,"I",115.63261711264397,"TON",8,{"v":0.5533036759302999,"d":"0.55"},{"$f":"VLOOKUP(A10660,cordwood_density!A:D,4,FALSE)","v":1.3963},{"v":0.39626418099999994,"d":"0.40"}]
["18031","18","IN","031","Decatur","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",147.43828162728,"A","CEC Survey",2017,15,"I",236.6960892236307,"TON",8,{"v":1.6053909921576002,"d":"1.61"},{"$f":"VLOOKUP(A10694,cordwood_density!A:D,4,FALSE)","v":1.3781},{"v":1.164930696,"d":"1.16"}]
["18035","18","IN","035","Delaware","","2104008100","Fireplace: general","Fireplace: general",3920.6633546559997,"A","CEC Survey",2017,15,"I",1638.287890472144,"TON",8,{"v":0.41785987274999997,"d":"0.42"},{"$f":"VLOOKUP(A10717,cordwood_density!A:D,4,FALSE)","v":1.381},{"v":0.30257775,"d":"0.30"}]
["18037","18","IN","037","Dubois","","2104009000","Wax Log; Total: All Combustor Types",null,265.0750396390586,"A","CEC Survey",2017,15,"I",147.8851778666146,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A10738,cordwood_density!A:D,4,FALSE)","v":1.4426},{"v":0.38673180056148615,"d":"0.39"}]
["18039","18","IN","039","Elkhart","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2674.05646077867,"A","CEC Survey",2017,15,"I",3578.920155153768,"TON",8,{"$f":"P10755/J10755","v":{"v":1.3383861588740003,"d":"1.34"}},{"$f":"VLOOKUP(A10755,cordwood_density!A:D,4,FALSE)","v":1.3297},{"$f":"S10755/T10755","v":{"v":1.00653242,"d":"1.01"}}]
["18043","18","IN","043","Floyd","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",556.1126304971999,"A","CEC Survey",2017,15,"I",429.58626210554,"TON",8,{"v":0.772480678458,"d":"0.77"},{"$f":"VLOOKUP(A10780,cordwood_density!A:D,4,FALSE)","v":1.4262},{"v":0.54163559,"d":"0.54"}]
["18045","18","IN","045","Fountain","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",203.84379637839,"A","CEC Survey",2017,15,"I",107.57431595859117,"TON",8,{"v":0.5277291625735999,"d":"0.53"},{"$f":"VLOOKUP(A10794,cordwood_density!A:D,4,FALSE)","v":1.3208},{"v":0.399552667,"d":"0.40"}]
["18051","18","IN","051","Gibson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.885577085388047,"A","CEC Survey",2017,15,"I",15.030395638889576,"TON",8,{"v":2.553767527096894,"d":"2.55"},{"$f":"VLOOKUP(A10833,cordwood_density!A:D,4,FALSE)","v":1.172},{"v":2.17898253165264,"d":"2.18"}]
["18053","18","IN","053","Grant","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3573.829865172,"A","CEC Survey",2017,15,"I",1195.0402563633702,"TON",8,{"v":0.3343864429612,"d":"0.33"},{"$f":"VLOOKUP(A10856,cordwood_density!A:D,4,FALSE)","v":1.3412},{"v":0.249318851,"d":"0.25"}]
["18055","18","IN","055","Greene","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",490.28331540500005,"A","CEC Survey",2017,15,"I",221.38960694848154,"TON",8,{"v":0.451554438,"d":"0.45"},{"$f":"VLOOKUP(A10872,cordwood_density!A:D,4,FALSE)","v":1.3816},{"v":0.3268344224088014,"d":"0.33"}]
["18059","18","IN","059","Hancock","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.518411279255483,"A","CEC Survey",2017,15,"I",35.60814493281902,"TON",8,{"v":3.0914111390473487,"d":"3.09"},{"$f":"VLOOKUP(A10893,cordwood_density!A:D,4,FALSE)","v":1.4298},{"v":2.1621283669375777,"d":"2.16"}]
["18061","18","IN","061","Harrison","","2104008610","Hydronic heater: outdoor","Hydronic heater",149.07021105812538,"A","CEC Survey",2017,15,"I",490.54449154484826,"TON",8,{"v":3.2906942846788847,"d":"3.29"},{"$f":"VLOOKUP(A10909,cordwood_density!A:D,4,FALSE)","v":1.4184},{"v":2.3200044308226766,"d":"2.32"}]
["18063","18","IN","063","Hendricks","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",318.60857041343996,"A","CEC Survey",2017,15,"I",162.0706251943358,"TON",8,{"v":0.508682566147,"d":"0.51"},{"$f":"VLOOKUP(A10928,cordwood_density!A:D,4,FALSE)","v":1.3258},{"v":0.383679715,"d":"0.38"}]
["18065","18","IN","065","Henry","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",220.81781240064,"A","CEC Survey",2017,15,"I",325.6688682917623,"TON",8,{"v":1.4748306069661,"d":"1.47"},{"$f":"VLOOKUP(A10949,cordwood_density!A:D,4,FALSE)","v":1.3207},{"v":1.1167037229999999,"d":"1.12"}]
["18071","18","IN","071","Jackson","","2104008620","Hydronic heater: indoor","Hydronic heater",64.05294886887565,"A","CEC Survey",2017,15,"I",201.89698996310725,"TON",8,{"v":3.1520327093201517,"d":"3.15"},{"$f":"VLOOKUP(A10985,cordwood_density!A:D,4,FALSE)","v":1.3929},{"v":2.262928214028395,"d":"2.26"}]
["18073","18","IN","073","Jasper","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1843.5795260999998,"A","CEC Survey",2017,15,"I",649.9463152313746,"TON",8,{"v":0.35254585225640006,"d":"0.35"},{"$f":"VLOOKUP(A11006,cordwood_density!A:D,4,FALSE)","v":1.4212},{"v":0.24806209700000004,"d":"0.25"}]
["18077","18","IN","077","Jefferson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",88.02372478458368,"A","CEC Survey",2017,15,"I",266.9911929693324,"TON",8,{"v":3.0331730862642705,"d":"3.03"},{"$f":"VLOOKUP(A11027,cordwood_density!A:D,4,FALSE)","v":1.3207},{"v":2.296640483277255,"d":"2.30"}]
["18077","18","IN","077","Jefferson","","2104009000","Wax Log; Total: All Combustor Types",null,203.36215671171303,"A","CEC Survey",2017,15,"I",113.45560395879166,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A11038,cordwood_density!A:D,4,FALSE)","v":1.3207},{"v":0.4224269671310668,"d":"0.42"}]
["18081","18","IN","081","Johnson","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,6956.06843685,"A","CEC Survey",2017,15,"I",2204.394893748136,"TON",8,{"v":0.31690241603580005,"d":"0.32"},{"$f":"VLOOKUP(A11066,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.256206982,"d":"0.26"}]
["18083","18","IN","083","Knox","","2104009000","Wax Log; Total: All Combustor Types",null,240.40271992440887,"A","CEC Survey",2017,15,"I",134.1205080797075,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A11083,cordwood_density!A:D,4,FALSE)","v":1.4009},{"v":0.3982434831108573,"d":"0.40"}]
["18087","18","IN","087","Lagrange","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",225.08515176576,"A","CEC Survey",2017,15,"I",367.5224421679018,"TON",8,{"v":1.6328151336716,"d":"1.63"},{"$f":"VLOOKUP(A11114,cordwood_density!A:D,4,FALSE)","v":1.2706},{"v":1.285074086,"d":"1.29"}]
["18091","18","IN","091","La Porte","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",423.228554064,"A","CEC Survey",2017,15,"I",614.0373026898997,"TON",8,{"v":1.4508409151359998,"d":"1.45"},{"$f":"VLOOKUP(A11144,cordwood_density!A:D,4,FALSE)","v":1.2928},{"v":1.1222469949999998,"d":"1.12"}]
["18093","18","IN","093","Lawrence","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",848.1158654976,"A","CEC Survey",2017,15,"I",1432.498319095345,"TON",8,{"v":1.689036106234,"d":"1.69"},{"$f":"VLOOKUP(A11161,cordwood_density!A:D,4,FALSE)","v":1.3939},{"v":1.2117340600000002,"d":"1.21"}]
["18097","18","IN","097","Marion","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",96.81700721860688,"A","CEC Survey",2017,15,"I",4.058067317227773,"TON",8,{"v":0.041914818829969676,"d":"0.04"},{"$f":"VLOOKUP(A11178,cordwood_density!A:D,4,FALSE)","v":1.4042},{"v":0.0298496074846672,"d":"0.03"}]
["18099","18","IN","099","Marshall","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",257.00608788259996,"A","CEC Survey",2017,15,"I",124.9793622394383,"TON",8,{"v":0.4862895010352,"d":"0.49"},{"$f":"VLOOKUP(A11200,cordwood_density!A:D,4,FALSE)","v":1.2641},{"v":0.384692272,"d":"0.38"}]
["18101","18","IN","101","Martin","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",166.86638615374653,"A","CEC Survey",2017,15,"I",103.91309528373256,"TON",8,{"v":0.622732341,"d":"0.62"},{"$f":"VLOOKUP(A11217,cordwood_density!A:D,4,FALSE)","v":1.3682},{"v":0.45514715757930124,"d":"0.46"}]
["18107","18","IN","107","Montgomery","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",248.11509464665002,"A","CEC Survey",2017,15,"I",114.85944558466902,"TON",8,{"v":0.4629280848399999,"d":"0.46"},{"$f":"VLOOKUP(A11260,cordwood_density!A:D,4,FALSE)","v":1.222},{"v":0.37882821999999994,"d":"0.38"}]
["18109","18","IN","109","Morgan","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3939.2498369899995,"A","CEC Survey",2017,15,"I",1167.4388804123394,"TON",8,{"v":0.2963607104708,"d":"0.30"},{"$f":"VLOOKUP(A11276,cordwood_density!A:D,4,FALSE)","v":1.1834},{"v":0.250431562,"d":"0.25"}]
["18111","18","IN","111","Newton","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",444.43867768930005,"A","CEC Survey",2017,15,"I",806.5296300286383,"TON",8,{"v":1.8147152138556002,"d":"1.81"},{"$f":"VLOOKUP(A11295,cordwood_density!A:D,4,FALSE)","v":1.4028},{"v":1.293637877,"d":"1.29"}]
["18115","18","IN","115","Ohio","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7932324345131925,"A","CEC Survey",2017,15,"I",2.450655171678512,"TON",8,{"v":3.089454068002756,"d":"3.09"},{"$f":"VLOOKUP(A11316,cordwood_density!A:D,4,FALSE)","v":1.3395},{"v":2.3064233430405046,"d":"2.31"}]
["18117","18","IN","117","Orange","","2104008610","Hydronic heater: outdoor","Hydronic heater",70.29147886521078,"A","CEC Survey",2017,15,"I",229.81477946159652,"TON",8,{"v":3.269454323222929,"d":"3.27"},{"$f":"VLOOKUP(A11329,cordwood_density!A:D,4,FALSE)","v":1.4265},{"v":2.291941341200791,"d":"2.29"}]
["18119","18","IN","119","Owen","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",835.2599179809401,"A","CEC Survey",2017,15,"I",1629.5270445225767,"TON",8,{"v":1.9509221135160002,"d":"1.95"},{"$f":"VLOOKUP(A11355,cordwood_density!A:D,4,FALSE)","v":1.3812},{"v":1.4124834300000002,"d":"1.41"}]
["18125","18","IN","125","Pike","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",175.24738745696,"A","CEC Survey",2017,15,"I",118.5488693156664,"TON",8,{"v":0.6764658294537,"d":"0.68"},{"$f":"VLOOKUP(A11394,cordwood_density!A:D,4,FALSE)","v":1.4157},{"v":0.477831341,"d":"0.48"}]
["18127","18","IN","127","Porter","","2104008620","Hydronic heater: indoor","Hydronic heater",188.5532316901792,"A","CEC Survey",2017,15,"I",564.75277917106,"TON",8,{"v":2.995190133357312,"d":"3.00"},{"$f":"VLOOKUP(A11405,cordwood_density!A:D,4,FALSE)","v":1.3923},{"v":2.1512534176235807,"d":"2.15"}]
["18131","18","IN","131","Pulaski","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.651290125732018,"A","CEC Survey",2017,15,"I",13.810524121395614,"TON",8,{"v":2.9691813987247504,"d":"2.97"},{"$f":"VLOOKUP(A11433,cordwood_density!A:D,4,FALSE)","v":1.2585},{"v":2.359301866289035,"d":"2.36"}]
["18133","18","IN","133","Putnam","","2104008620","Hydronic heater: indoor","Hydronic heater",78.52373161623484,"A","CEC Survey",2017,15,"I",262.6842882702787,"TON",8,{"v":3.3452853406672354,"d":"3.35"},{"$f":"VLOOKUP(A11450,cordwood_density!A:D,4,FALSE)","v":1.4301},{"v":2.3391967978933192,"d":"2.34"}]
["18137","18","IN","137","Ripley","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.7993110334650693,"A","CEC Survey",2017,15,"I",8.951391619227188,"TON",8,{"v":3.197712405736812,"d":"3.20"},{"$f":"VLOOKUP(A11481,cordwood_density!A:D,4,FALSE)","v":1.4136},{"v":2.2621055501816723,"d":"2.26"}]
["18137","18","IN","137","Ripley","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",194.47174379999998,"A","CEC Survey",2017,15,"I",349.86985801516636,"TON",8,{"v":1.7990781137592,"d":"1.80"},{"$f":"VLOOKUP(A11489,cordwood_density!A:D,4,FALSE)","v":1.4136},{"v":1.272692497,"d":"1.27"}]
["18143","18","IN","143","Scott","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",74.78984514550908,"A","CEC Survey",2017,15,"I",50.59300719600246,"TON",8,{"v":0.6764689390327001,"d":"0.68"},{"$f":"VLOOKUP(A11528,cordwood_density!A:D,4,FALSE)","v":1.3673},{"v":0.4947479990000001,"d":"0.49"}]
["18145","18","IN","145","Shelby","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2524.4053382310003,"A","CEC Survey",2017,15,"I",833.2399528143013,"TON",8,{"v":0.33007375645869996,"d":"0.33"},{"$f":"VLOOKUP(A11546,cordwood_density!A:D,4,FALSE)","v":1.3207},{"v":0.24992334099999997,"d":"0.25"}]
["18149","18","IN","149","Starke","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",95.18634666701378,"A","CEC Survey",2017,15,"I",282.0633405581297,"TON",8,{"v":2.963275201062811,"d":"2.96"},{"$f":"VLOOKUP(A11567,cordwood_density!A:D,4,FALSE)","v":1.3019},{"v":2.276115831525318,"d":"2.28"}]
["18151","18","IN","151","Steuben","","2104008610","Hydronic heater: outdoor","Hydronic heater",127.43284343206882,"A","CEC Survey",2017,15,"I",422.29033814275476,"TON",8,{"v":3.313826536154056,"d":"3.31"},{"$f":"VLOOKUP(A11584,cordwood_density!A:D,4,FALSE)","v":1.4338},{"v":2.311219511894306,"d":"2.31"}]
["18153","18","IN","153","Sullivan","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",150.95839227315,"A","CEC Survey",2017,15,"I",86.62094537641806,"TON",8,{"v":0.5738067561006,"d":"0.57"},{"$f":"VLOOKUP(A11605,cordwood_density!A:D,4,FALSE)","v":1.3921},{"v":0.412187886,"d":"0.41"}]
["18155","18","IN","155","Switzerland","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",131.51485160345,"A","CEC Survey",2017,15,"I",111.9232381039256,"TON",8,{"v":0.8510311705433999,"d":"0.85"},{"$f":"VLOOKUP(A11620,cordwood_density!A:D,4,FALSE)","v":1.4133},{"v":0.602158898,"d":"0.60"}]
["18159","18","IN","159","Tipton","","2104008610","Hydronic heater: outdoor","Hydronic heater",44.75024628707595,"A","CEC Survey",2017,15,"I",131.20586539024768,"TON",8,{"v":2.9319585092013325,"d":"2.93"},{"$f":"VLOOKUP(A11644,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2543122475790653,"d":"2.25"}]
["18163","18","IN","163","Vanderburgh","","2104009000","Wax Log; Total: All Combustor Types",null,1201.9013067191017,"A","CEC Survey",2017,15,"I",670.5398922670972,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A11683,cordwood_density!A:D,4,FALSE)","v":1.3713},{"v":0.4068397108510173,"d":"0.41"}]
["18165","18","IN","165","Vermillion","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1008.782781398,"A","CEC Survey",2017,15,"I",360.7286513205111,"TON",8,{"v":0.35758803378919995,"d":"0.36"},{"$f":"VLOOKUP(A11696,cordwood_density!A:D,4,FALSE)","v":1.4239},{"v":0.251132828,"d":"0.25"}]
["18169","18","IN","169","Wabash","","2104008100","Fireplace: general","Fireplace: general",1037.76441316,"A","CEC Survey",2017,15,"I",468.0446138793943,"TON",8,{"v":0.4510123954377999,"d":"0.45"},{"$f":"VLOOKUP(A11722,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.3467725629999999,"d":"0.35"}]
["18171","18","IN","171","Warren","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",121.46183073885,"A","CEC Survey",2017,15,"I",60.5555808965019,"TON",8,{"v":0.4985564644312,"d":"0.50"},{"$f":"VLOOKUP(A11739,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.38332805200000003,"d":"0.38"}]
["18175","18","IN","175","Washington","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",417.04486754,"A","CEC Survey",2017,15,"I",233.04934663727227,"TON",8,{"v":0.558811209,"d":"0.56"},{"$f":"VLOOKUP(A11772,cordwood_density!A:D,4,FALSE)","v":1.4819},{"v":0.3770910378568055,"d":"0.38"}]
["18177","18","IN","177","Wayne","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.617189281853452,"A","CEC Survey",2017,15,"I",33.022177696345445,"TON",8,{"v":2.8425273011542904,"d":"2.84"},{"$f":"VLOOKUP(A11778,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.1855507466971327,"d":"2.19"}]
["18181","18","IN","181","White","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",403.5488757304954,"A","CEC Survey",2017,15,"I",161.43343761965866,"TON",8,{"v":0.400034413,"d":"0.40"},{"$f":"VLOOKUP(A11817,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.3075768206981393,"d":"0.31"}]
["19001","19","IA","001","Adair","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",41.942646296251766,"A","CEC Survey",2017,15,"I",95.66000585298298,"TON",8,{"v":2.280733675631995,"d":"2.28"},{"$f":"VLOOKUP(A11837,cordwood_density!A:D,4,FALSE)","v":1.3268},{"v":1.7189732255290888,"d":"1.72"}]
["19003","19","IA","003","Adams","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.6388604423789658,"A","CEC Survey",2017,15,"I",1.4319261989911822,"TON",8,{"v":2.2413755869106975,"d":"2.24"},{"$f":"VLOOKUP(A11856,cordwood_density!A:D,4,FALSE)","v":1.293},{"v":1.7334691314081188,"d":"1.73"}]
["19005","19","IA","005","Allamakee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",44.444265766758015,"A","CEC Survey",2017,15,"I",18.946959062060547,"TON",8,{"v":0.4263082927614001,"d":"0.43"},{"$f":"VLOOKUP(A11873,cordwood_density!A:D,4,FALSE)","v":1.3329},{"v":0.31983516600000006,"d":"0.32"}]
["19007","19","IA","007","Appanoose","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",105.75191328975001,"A","CEC Survey",2017,15,"I",40.99805123748605,"TON",8,{"v":0.3876814136228,"d":"0.39"},{"$f":"VLOOKUP(A11890,cordwood_density!A:D,4,FALSE)","v":1.3541},{"v":0.286301908,"d":"0.29"}]
["19011","19","IA","011","Benton","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",127.48964268962762,"A","CEC Survey",2017,15,"I",296.21967495296394,"TON",8,{"v":2.323480313409522,"d":"2.32"},{"$f":"VLOOKUP(A11912,cordwood_density!A:D,4,FALSE)","v":1.351},{"v":1.719822585795353,"d":"1.72"}]
["19015","19","IA","015","Boone","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1564.881631326,"A","CEC Survey",2017,15,"I",392.63045812203273,"TON",8,{"v":0.25090105875249996,"d":"0.25"},{"$f":"VLOOKUP(A11951,cordwood_density!A:D,4,FALSE)","v":1.3897},{"v":0.18054332499999998,"d":"0.18"}]
["19017","19","IA","017","Bremer","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1443.7379918800002,"A","CEC Survey",2017,15,"I",340.99802008539706,"TON",8,{"v":0.23619106929600003,"d":"0.24"},{"$f":"VLOOKUP(A11966,cordwood_density!A:D,4,FALSE)","v":1.308},{"v":0.180574212,"d":"0.18"}]
["19021","19","IA","021","Buena Vista","","2104008620","Hydronic heater: indoor","Hydronic heater",52.451047971358214,"A","CEC Survey",2017,15,"I",127.45719577703511,"TON",8,{"v":2.4300219100795712,"d":"2.43"},{"$f":"VLOOKUP(A11990,cordwood_density!A:D,4,FALSE)","v":1.3686},{"v":1.7755530542741278,"d":"1.78"}]
["19023","19","IA","023","Butler","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1033.18467967,"A","CEC Survey",2017,15,"I",243.73358566114223,"TON",8,{"v":0.2359051488636,"d":"0.24"},{"$f":"VLOOKUP(A12011,cordwood_density!A:D,4,FALSE)","v":1.3017},{"v":0.18122850799999998,"d":"0.18"}]
["19025","19","IA","025","Calhoun","","2104009000","Wax Log; Total: All Combustor Types",null,67.84085830510644,"A","CEC Survey",2017,15,"I",52.94940999832906,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A12028,cordwood_density!A:D,4,FALSE)","v":1.0253},{"v":0.7612351506876035,"d":"0.76"}]
["19031","19","IA","031","Cedar","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.656897431021392,"A","CEC Survey",2017,15,"I",17.874876240918407,"TON",8,{"v":2.3344803037976685,"d":"2.33"},{"$f":"VLOOKUP(A12063,cordwood_density!A:D,4,FALSE)","v":1.3577},{"v":1.7194375074005073,"d":"1.72"}]
["19031","19","IA","031","Cedar","","2104008100","Fireplace: general","Fireplace: general",530.4546875320001,"A","CEC Survey",2017,15,"I",199.97155005596758,"TON",8,{"v":0.376981398706,"d":"0.38"},{"$f":"VLOOKUP(A12067,cordwood_density!A:D,4,FALSE)","v":1.3577},{"v":0.27766178,"d":"0.28"}]
["19035","19","IA","035","Cherokee","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",278.7442004746,"A","CEC Survey",2017,15,"I",347.01242795340187,"TON",8,{"v":1.2449135349276,"d":"1.24"},{"$f":"VLOOKUP(A12106,cordwood_density!A:D,4,FALSE)","v":1.3646},{"v":0.9122919059999999,"d":"0.91"}]
["19039","19","IA","039","Clarke","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",25.396102238399997,"A","CEC Survey",2017,15,"I",9.58471632817788,"TON",8,{"v":0.3774089519014999,"d":"0.38"},{"$f":"VLOOKUP(A12128,cordwood_density!A:D,4,FALSE)","v":1.3355},{"v":0.282597493,"d":"0.28"}]
["19041","19","IA","041","Clay","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",109.6192294288,"A","CEC Survey",2017,15,"I",35.13888356390291,"TON",8,{"v":0.3205540099762,"d":"0.32"},{"$f":"VLOOKUP(A12145,cordwood_density!A:D,4,FALSE)","v":1.3013},{"v":0.246333674,"d":"0.25"}]
["19043","19","IA","043","Clayton","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",359.616388125,"A","CEC Survey",2017,15,"I",233.4326762343224,"TON",8,{"v":0.649115791,"d":"0.65"},{"$f":"VLOOKUP(A12162,cordwood_density!A:D,4,FALSE)","v":1.3505},{"v":0.48064849389115144,"d":"0.48"}]
["19045","19","IA","045","Clinton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",684.7622296014499,"A","CEC Survey",2017,15,"I",711.4155583809612,"TON",8,{"v":1.0389234797530003,"d":"1.04"},{"$f":"VLOOKUP(A12181,cordwood_density!A:D,4,FALSE)","v":1.283},{"v":0.8097610910000003,"d":"0.81"}]
["19049","19","IA","049","Dallas","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.722436233438901,"A","CEC Survey",2017,15,"I",13.574170218772549,"TON",8,{"v":2.372096370327773,"d":"2.37"},{"$f":"VLOOKUP(A12201,cordwood_density!A:D,4,FALSE)","v":1.3566},{"v":1.7485599073623566,"d":"1.75"}]
["19053","19","IA","053","Decatur","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",280.3914635548042,"A","CEC Survey",2017,15,"I",358.2301055387253,"TON",8,{"v":1.2776070319584,"d":"1.28"},{"$f":"VLOOKUP(A12240,cordwood_density!A:D,4,FALSE)","v":1.3116},{"v":0.974082824,"d":"0.97"}]
["19057","19","IA","057","Des Moines","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",102.26660551221508,"A","CEC Survey",2017,15,"I",228.76438138294617,"TON",8,{"v":2.2369411817000393,"d":"2.24"},{"$f":"VLOOKUP(A12257,cordwood_density!A:D,4,FALSE)","v":1.3502},{"v":1.6567480237742847,"d":"1.66"}]
["19059","19","IA","059","Dickinson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",169.57016247181,"A","CEC Survey",2017,15,"I",54.77789222055645,"TON",8,{"v":0.32303968706560005,"d":"0.32"},{"$f":"VLOOKUP(A12279,cordwood_density!A:D,4,FALSE)","v":1.3568},{"v":0.23808939200000004,"d":"0.24"}]
["19061","19","IA","061","Dubuque","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1861.6348256954402,"A","CEC Survey",2017,15,"I",2129.0953301741433,"TON",8,{"v":1.1436696933185,"d":"1.14"},{"$f":"VLOOKUP(A12300,cordwood_density!A:D,4,FALSE)","v":1.3891},{"v":0.823317035,"d":"0.82"}]
["19063","19","IA","063","Emmet","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",63.14116686639999,"A","CEC Survey",2017,15,"I",19.945172833246783,"TON",8,{"v":0.31588223378020003,"d":"0.32"},{"$f":"VLOOKUP(A12310,cordwood_density!A:D,4,FALSE)","v":1.2994},{"v":0.243098533,"d":"0.24"}]
["19067","19","IA","067","Floyd","","2104008620","Hydronic heater: indoor","Hydronic heater",52.126375316309655,"A","CEC Survey",2017,15,"I",127.77251740997053,"TON",8,{"v":2.451206642215773,"d":"2.45"},{"$f":"VLOOKUP(A12335,cordwood_density!A:D,4,FALSE)","v":1.3708},{"v":1.7881577489172549,"d":"1.79"}]
["19069","19","IA","069","Franklin","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,666.674547976,"A","CEC Survey",2017,15,"I",157.78277925148487,"TON",8,{"v":0.23667137095680002,"d":"0.24"},{"$f":"VLOOKUP(A12356,cordwood_density!A:D,4,FALSE)","v":1.3056},{"v":0.181274028,"d":"0.18"}]
["19073","19","IA","073","Greene","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,612.7458938753676,"A","CEC Survey",2017,15,"I",143.03335894555013,"TON",8,{"v":0.233430138619,"d":"0.23"},{"$f":"VLOOKUP(A12386,cordwood_density!A:D,4,FALSE)","v":1.2898},{"v":0.180981655,"d":"0.18"}]
["19077","19","IA","077","Guthrie","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",24.91480039392,"A","CEC Survey",2017,15,"I",9.09688588841582,"TON",8,{"v":0.36511975791850004,"d":"0.37"},{"$f":"VLOOKUP(A12413,cordwood_density!A:D,4,FALSE)","v":1.3663},{"v":0.267232495,"d":"0.27"}]
["19079","19","IA","079","Hamilton","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",89.28593215139999,"A","CEC Survey",2017,15,"I",106.11355162247996,"TON",8,{"v":1.1884688781940003,"d":"1.19"},{"$f":"VLOOKUP(A12434,cordwood_density!A:D,4,FALSE)","v":1.378},{"v":0.8624592730000002,"d":"0.86"}]
["19081","19","IA","081","Hancock","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",255.8489561271,"A","CEC Survey",2017,15,"I",305.09589578370407,"TON",8,{"v":1.1924844267574002,"d":"1.19"},{"$f":"VLOOKUP(A12451,cordwood_density!A:D,4,FALSE)","v":1.2838},{"v":0.9288708730000002,"d":"0.93"}]
["19085","19","IA","085","Harrison","","2104008100","Fireplace: general","Fireplace: general",388.25542778,"A","CEC Survey",2017,15,"I",139.13660894298218,"TON",8,{"v":0.35836359001740004,"d":"0.36"},{"$f":"VLOOKUP(A12472,cordwood_density!A:D,4,FALSE)","v":1.3123},{"v":0.27308053800000004,"d":"0.27"}]
["19087","19","IA","087","Henry","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",125.5550826564452,"A","CEC Survey",2017,15,"I",47.26502542856946,"TON",8,{"v":0.376448523059,"d":"0.38"},{"$f":"VLOOKUP(A12490,cordwood_density!A:D,4,FALSE)","v":1.387},{"v":0.271412057,"d":"0.27"}]
["19093","19","IA","093","Ida","","2104008610","Hydronic heater: outdoor","Hydronic heater",46.118051299804954,"A","CEC Survey",2017,15,"I",81.12417894745482,"TON",8,{"v":1.759054787898159,"d":"1.76"},{"$f":"VLOOKUP(A12529,cordwood_density!A:D,4,FALSE)","v":1.003},{"v":1.7537934076751338,"d":"1.75"}]
["19095","19","IA","095","Iowa","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",36.93927145632,"A","CEC Survey",2017,15,"I",12.557743098880081,"TON",8,{"v":0.339956436708,"d":"0.34"},{"$f":"VLOOKUP(A12548,cordwood_density!A:D,4,FALSE)","v":1.302},{"v":0.261103254,"d":"0.26"}]
["19097","19","IA","097","Jackson","","2104009000","Wax Log; Total: All Combustor Types",null,134.67108192749316,"A","CEC Survey",2017,15,"I",105.11002528634961,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A12568,cordwood_density!A:D,4,FALSE)","v":1.3244},{"v":0.5893192389006342,"d":"0.59"}]
["19101","19","IA","101","Jefferson","","2104008610","Hydronic heater: outdoor","Hydronic heater",48.955744015596935,"A","CEC Survey",2017,15,"I",113.13957882524014,"TON",8,{"v":2.311058305828111,"d":"2.31"},{"$f":"VLOOKUP(A12589,cordwood_density!A:D,4,FALSE)","v":1.3653},{"v":1.692710983540695,"d":"1.69"}]
["19101","19","IA","101","Jefferson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",257.263751696,"A","CEC Survey",2017,15,"I",297.44632871708916,"TON",8,{"v":1.1561921442729002,"d":"1.16"},{"$f":"VLOOKUP(A12601,cordwood_density!A:D,4,FALSE)","v":1.3653},{"v":0.8468410930000002,"d":"0.85"}]
["19105","19","IA","105","Jones","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",226.08709048,"A","CEC Survey",2017,15,"I",81.11986263369674,"TON",8,{"v":0.358799179827,"d":"0.36"},{"$f":"VLOOKUP(A12624,cordwood_density!A:D,4,FALSE)","v":1.3222},{"v":0.271365285,"d":"0.27"}]
["19107","19","IA","107","Keokuk","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",429.77010605256,"A","CEC Survey",2017,15,"I",538.1817215326131,"TON",8,{"v":1.2522549008255,"d":"1.25"},{"$f":"VLOOKUP(A12645,cordwood_density!A:D,4,FALSE)","v":1.3145},{"v":0.952647319,"d":"0.95"}]
["19113","19","IA","113","Linn","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",414.7552112554278,"A","CEC Survey",2017,15,"I",928.0898446780174,"TON",8,{"v":2.2376809729979534,"d":"2.24"},{"$f":"VLOOKUP(A12677,cordwood_density!A:D,4,FALSE)","v":1.3599},{"v":1.6454746473990391,"d":"1.65"}]
["19115","19","IA","115","Louisa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",211.981483288,"A","CEC Survey",2017,15,"I",85.14418495545554,"TON",8,{"v":0.40165859600000003,"d":"0.40"},{"$f":"VLOOKUP(A12702,cordwood_density!A:D,4,FALSE)","v":1.2419},{"v":0.3234226556083421,"d":"0.32"}]
["19119","19","IA","119","Lyon","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.436166331355619,"A","CEC Survey",2017,15,"I",18.249462964121193,"TON",8,{"v":2.454149376294855,"d":"2.45"},{"$f":"VLOOKUP(A12723,cordwood_density!A:D,4,FALSE)","v":1.3481},{"v":1.8204505424633595,"d":"1.82"}]
["19123","19","IA","123","Mahaska","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.384157924724303,"A","CEC Survey",2017,15,"I",11.885098803892843,"TON",8,{"v":2.2074201704440943,"d":"2.21"},{"$f":"VLOOKUP(A12753,cordwood_density!A:D,4,FALSE)","v":1.3217},{"v":1.670137073801993,"d":"1.67"}]
["19123","19","IA","123","Mahaska","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",317.3573196354391,"A","CEC Survey",2017,15,"I",95.41343943080177,"TON",8,{"v":0.300649878,"d":"0.30"},{"$f":"VLOOKUP(A12762,cordwood_density!A:D,4,FALSE)","v":1.3217},{"v":0.22747210259514258,"d":"0.23"}]
["19125","19","IA","125","Marion","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",169.46667909791998,"A","CEC Survey",2017,15,"I",198.8844507994076,"TON",8,{"v":1.1735903002176,"d":"1.17"},{"$f":"VLOOKUP(A12779,cordwood_density!A:D,4,FALSE)","v":1.3752},{"v":0.853396088,"d":"0.85"}]
["19129","19","IA","129","Mills","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,865.3888563794937,"A","CEC Survey",2017,15,"I",203.9836591948596,"TON",8,{"v":0.23571329546380002,"d":"0.24"},{"$f":"VLOOKUP(A12806,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.181234273,"d":"0.18"}]
["19133","19","IA","133","Monona","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",351.27470980755,"A","CEC Survey",2017,15,"I",426.7003115817617,"TON",8,{"v":1.2147197041755,"d":"1.21"},{"$f":"VLOOKUP(A12840,cordwood_density!A:D,4,FALSE)","v":1.3155},{"v":0.9233901210000001,"d":"0.92"}]
["19137","19","IA","137","Montgomery","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",38.047059956869255,"A","CEC Survey",2017,15,"I",82.83129374600108,"TON",8,{"v":2.1770747553135497,"d":"2.18"},{"$f":"VLOOKUP(A12857,cordwood_density!A:D,4,FALSE)","v":1.2999},{"v":1.6748017196042384,"d":"1.67"}]
["19139","19","IA","139","Muscatine","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",74.88994978872,"A","CEC Survey",2017,15,"I",26.308162760366493,"TON",8,{"v":0.3512909654044,"d":"0.35"},{"$f":"VLOOKUP(A12878,cordwood_density!A:D,4,FALSE)","v":1.3196},{"v":0.266210189,"d":"0.27"}]
["19141","19","IA","141","Obrien","","2104008100","Fireplace: general","Fireplace: general",428.821914352,"A","CEC Survey",2017,15,"I",125.75891072752992,"TON",8,{"v":0.2932660540858,"d":"0.29"},{"$f":"VLOOKUP(A12892,cordwood_density!A:D,4,FALSE)","v":1.1146},{"v":0.263113273,"d":"0.26"}]
["19143","19","IA","143","Osceola","","2104009000","Wax Log; Total: All Combustor Types",null,41.981443883770055,"A","CEC Survey",2017,15,"I",32.76628185519677,"TON",8,{"v":0.7804943999999998,"d":"0.78"},{"$f":"VLOOKUP(A12913,cordwood_density!A:D,4,FALSE)","v":1.1481},{"v":0.679813953488372,"d":"0.68"}]
["19149","19","IA","149","Plymouth","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1562.148814593,"A","CEC Survey",2017,15,"I",373.6192230891645,"TON",8,{"v":0.23917005831899998,"d":"0.24"},{"$f":"VLOOKUP(A12956,cordwood_density!A:D,4,FALSE)","v":1.3219},{"v":0.18092900999999997,"d":"0.18"}]
["19151","19","IA","151","Pocahontas","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",19.29586263456,"A","CEC Survey",2017,15,"I",5.231114790604383,"TON",8,{"v":0.2711003332515,"d":"0.27"},{"$f":"VLOOKUP(A12968,cordwood_density!A:D,4,FALSE)","v":1.1195},{"v":0.24216197700000003,"d":"0.24"}]
["19153","19","IA","153","Polk","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",4306.037783432,"A","CEC Survey",2017,15,"I",3497.948945772891,"TON",8,{"v":0.8123358692373002,"d":"0.81"},{"$f":"VLOOKUP(A12991,cordwood_density!A:D,4,FALSE)","v":1.2543},{"v":0.6476408110000001,"d":"0.65"}]
["19157","19","IA","157","Poweshiek","","2104008100","Fireplace: general","Fireplace: general",488.21600313899995,"A","CEC Survey",2017,15,"I",171.05977734661863,"TON",8,{"v":0.3503772433652,"d":"0.35"},{"$f":"VLOOKUP(A13012,cordwood_density!A:D,4,FALSE)","v":1.3729},{"v":0.255209588,"d":"0.26"}]
["19161","19","IA","161","Sac","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",117.22127791440002,"A","CEC Survey",2017,15,"I",37.054819180900665,"TON",8,{"v":0.3161100086962,"d":"0.32"},{"$f":"VLOOKUP(A13044,cordwood_density!A:D,4,FALSE)","v":1.2911},{"v":0.244837742,"d":"0.24"}]
["19161","19","IA","161","Sac","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",269.6391923064,"A","CEC Survey",2017,15,"I",333.0024472473618,"TON",8,{"v":1.2349927486393002,"d":"1.23"},{"$f":"VLOOKUP(A13051,cordwood_density!A:D,4,FALSE)","v":1.2911},{"v":0.9565430630000002,"d":"0.96"}]
["19167","19","IA","167","Sioux","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",198.1649952254,"A","CEC Survey",2017,15,"I",50.83706243949516,"TON",8,{"v":0.25653906423620004,"d":"0.26"},{"$f":"VLOOKUP(A13090,cordwood_density!A:D,4,FALSE)","v":1.0558},{"v":0.24298073900000003,"d":"0.24"}]
["19169","19","IA","169","Story","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",159.43701570783324,"A","CEC Survey",2017,15,"I",369.3875150327403,"TON",8,{"v":2.31682406618573,"d":"2.32"},{"$f":"VLOOKUP(A13097,cordwood_density!A:D,4,FALSE)","v":1.3845},{"v":1.6734012756848897,"d":"1.67"}]
["19173","19","IA","173","Taylor","","2104008610","Hydronic heater: outdoor","Hydronic heater",38.77524601931085,"A","CEC Survey",2017,15,"I",89.25374487659496,"TON",8,{"v":2.301822787459422,"d":"2.30"},{"$f":"VLOOKUP(A13129,cordwood_density!A:D,4,FALSE)","v":1.3125},{"v":1.7537697428262264,"d":"1.75"}]
["19175","19","IA","175","Union","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0278301217442702,"A","CEC Survey",2017,15,"I",2.28181366774827,"TON",8,{"v":2.220029963585751,"d":"2.22"},{"$f":"VLOOKUP(A13146,cordwood_density!A:D,4,FALSE)","v":1.3115},{"v":1.6927411083383537,"d":"1.69"}]
["19179","19","IA","179","Wapello","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.899895553494109,"A","CEC Survey",2017,15,"I",17.984451861977785,"TON",8,{"v":2.276542992270739,"d":"2.28"},{"$f":"VLOOKUP(A13173,cordwood_density!A:D,4,FALSE)","v":1.3762},{"v":1.654223944390887,"d":"1.65"}]
["19179","19","IA","179","Wapello","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",737.33419966844,"A","CEC Survey",2017,15,"I",829.5426519683779,"TON",8,{"v":1.1250565243568,"d":"1.13"},{"$f":"VLOOKUP(A13185,cordwood_density!A:D,4,FALSE)","v":1.3762},{"v":0.817509464,"d":"0.82"}]
["19185","19","IA","185","Wayne","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",83.259044769,"A","CEC Survey",2017,15,"I",29.753121368871113,"TON",8,{"v":0.35735602602000005,"d":"0.36"},{"$f":"VLOOKUP(A13224,cordwood_density!A:D,4,FALSE)","v":1.3425},{"v":0.266186984,"d":"0.27"}]
["19187","19","IA","187","Webster","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",68.99168572295999,"A","CEC Survey",2017,15,"I",24.681775402498808,"TON",8,{"v":0.35774999761000004,"d":"0.36"},{"$f":"VLOOKUP(A13238,cordwood_density!A:D,4,FALSE)","v":1.39},{"v":0.257374099,"d":"0.26"}]
["19191","19","IA","191","Winneshiek","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",9.545936545487264,"A","CEC Survey",2017,15,"I",23.286566343746163,"TON",8,{"v":2.4394218663389955,"d":"2.44"},{"$f":"VLOOKUP(A13263,cordwood_density!A:D,4,FALSE)","v":1.3516},{"v":1.8048400905142021,"d":"1.80"}]
["19193","19","IA","193","Woodbury","","2104008620","Hydronic heater: indoor","Hydronic heater",151.02040541971795,"A","CEC Survey",2017,15,"I",352.02338415647733,"TON",8,{"v":2.3309656941929746,"d":"2.33"},{"$f":"VLOOKUP(A13280,cordwood_density!A:D,4,FALSE)","v":1.3681},{"v":1.7037977444579888,"d":"1.70"}]
["19195","19","IA","195","Worth","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,529.329923848,"A","CEC Survey",2017,15,"I",128.6582989422754,"TON",8,{"v":0.2430588053798,"d":"0.24"},{"$f":"VLOOKUP(A13301,cordwood_density!A:D,4,FALSE)","v":1.3414},{"v":0.18119785700000002,"d":"0.18"}]
["20001","20","KS","001","Allen","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",273.4471956648984,"A","CEC Survey",2017,15,"I",391.07970253269843,"TON",8,{"v":1.4301836286225997,"d":"1.43"},{"$f":"VLOOKUP(A13335,cordwood_density!A:D,4,FALSE)","v":1.2458},{"v":1.1480041969999997,"d":"1.15"}]
["20003","20","KS","003","Anderson","","2104008620","Hydronic heater: indoor","Hydronic heater",13.154588324606852,"A","CEC Survey",2017,15,"I",36.64726706427172,"TON",8,{"v":2.785892356336206,"d":"2.79"},{"$f":"VLOOKUP(A13340,cordwood_density!A:D,4,FALSE)","v":1.2457},{"v":2.236407125580963,"d":"2.24"}]
["20007","20","KS","007","Barber","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",27.008214894069333,"A","CEC Survey",2017,15,"I",38.81052045251287,"TON",8,{"$f":"P13379/J13379","v":{"v":1.4369894717120002,"d":"1.44"}},{"$f":"VLOOKUP(A13379,cordwood_density!A:D,4,FALSE)","v":1.1584},{"$f":"S13379/T13379","v":{"v":1.240495055,"d":"1.24"}}]
["20009","20","KS","009","Barton","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",53.279860735679996,"A","CEC Survey",2017,15,"I",20.878600980034783,"TON",8,{"v":0.3918666582785,"d":"0.39"},{"$f":"VLOOKUP(A13388,cordwood_density!A:D,4,FALSE)","v":1.1567},{"v":0.33877985499999996,"d":"0.34"}]
["20013","20","KS","013","Brown","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",21.580110527044486,"A","CEC Survey",2017,15,"I",9.458284350200147,"TON",8,{"v":0.4382871134208,"d":"0.44"},{"$f":"VLOOKUP(A13418,cordwood_density!A:D,4,FALSE)","v":1.2288},{"v":0.35667896600000004,"d":"0.36"}]
["20015","20","KS","015","Butler","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",374.94557539746876,"A","CEC Survey",2017,15,"I",160.57227179726118,"TON",8,{"v":0.4282548783968,"d":"0.43"},{"$f":"VLOOKUP(A13435,cordwood_density!A:D,4,FALSE)","v":1.2124},{"v":0.353229032,"d":"0.35"}]
["20019","20","KS","019","Chautauqua","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",40.25767617952,"A","CEC Survey",2017,15,"I",22.60047195301791,"TON",8,{"v":0.5613953436417,"d":"0.56"},{"$f":"VLOOKUP(A13464,cordwood_density!A:D,4,FALSE)","v":1.4163},{"v":0.396381659,"d":"0.40"}]
["20021","20","KS","021","Cherokee","","2104008610","Hydronic heater: outdoor","Hydronic heater",40.992850081103796,"A","CEC Survey",2017,15,"I",110.24292080485439,"TON",8,{"v":2.68932071292287,"d":"2.69"},{"$f":"VLOOKUP(A13474,cordwood_density!A:D,4,FALSE)","v":1.2321},{"v":2.182713020796096,"d":"2.18"}]
["20025","20","KS","025","Clark","","2104009000","Wax Log; Total: All Combustor Types",null,14.630140168895029,"A","CEC Survey",2017,15,"I",2.0482196236453043,"TON",8,0.14,{"$f":"VLOOKUP(A13513,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.10764262648008613,"d":"0.11"}]
["20027","20","KS","027","Clay","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",43.406708551440005,"A","CEC Survey",2017,15,"I",60.995678771273404,"TON",8,{"v":1.4052131757234998,"d":"1.41"},{"$f":"VLOOKUP(A13529,cordwood_density!A:D,4,FALSE)","v":1.2389},{"v":1.134242615,"d":"1.13"}]
["20031","20","KS","031","Coffey","","2104008100","Fireplace: general","Fireplace: general",249.563643368,"A","CEC Survey",2017,15,"I",125.16325647751454,"TON",8,{"v":0.501528406896,"d":"0.50"},{"$f":"VLOOKUP(A13552,cordwood_density!A:D,4,FALSE)","v":1.304},{"v":0.38460767399999995,"d":"0.38"}]
["20033","20","KS","033","Comanche","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",19.137570452880002,"A","CEC Survey",2017,15,"I",8.720114039133378,"TON",8,{"v":0.4556541835132,"d":"0.46"},{"$f":"VLOOKUP(A13569,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.35034152199999996,"d":"0.35"}]
["20035","20","KS","035","Cowley","","2104008100","Fireplace: general","Fireplace: general",1159.289035536,"A","CEC Survey",2017,15,"I",499.35187490956883,"TON",8,{"v":0.4307397548004,"d":"0.43"},{"$f":"VLOOKUP(A13582,cordwood_density!A:D,4,FALSE)","v":1.2249},{"v":0.351652996,"d":"0.35"}]
["20039","20","KS","039","Decatur","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.1532769045654445,"A","CEC Survey",2017,15,"I",3.344308244664959,"TON",8,{"v":2.8998311085793365,"d":"2.90"},{"$f":"VLOOKUP(A13608,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2296102634009967,"d":"2.23"}]
["20041","20","KS","041","Dickinson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",181.77644643243,"A","CEC Survey",2017,15,"I",78.43705577140135,"TON",8,{"v":0.4315028559025,"d":"0.43"},{"$f":"VLOOKUP(A13629,cordwood_density!A:D,4,FALSE)","v":1.2343},{"v":0.349593175,"d":"0.35"}]
["20045","20","KS","045","Douglas","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",160.89513754380002,"A","CEC Survey",2017,15,"I",81.11725547435904,"TON",8,{"v":0.5041622556944999,"d":"0.50"},{"$f":"VLOOKUP(A13658,cordwood_density!A:D,4,FALSE)","v":1.2051},{"v":0.4183571949999999,"d":"0.42"}]
["20049","20","KS","049","Elk","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.23663994064544855,"A","CEC Survey",2017,15,"I",0.7154447740276965,"TON",8,{"v":3.0233475045517726,"d":"3.02"},{"$f":"VLOOKUP(A13686,cordwood_density!A:D,4,FALSE)","v":1.4289},{"v":2.1158566061668225,"d":"2.12"}]
["20051","20","KS","051","Ellis","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",328.218970673,"A","CEC Survey",2017,15,"I",76.11112510689972,"TON",8,{"v":0.23189130399999996,"d":"0.23"},{"$f":"VLOOKUP(A13707,cordwood_density!A:D,4,FALSE)","v":1.2702},{"v":0.1825628279011179,"d":"0.18"}]
["20053","20","KS","053","Ellsworth","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",30.2249484,"A","CEC Survey",2017,15,"I",45.86778434448948,"TON",8,{"v":1.5175471513621999,"d":"1.52"},{"$f":"VLOOKUP(A13724,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.1668054369999998,"d":"1.17"}]
["20057","20","KS","057","Ford","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",386.66686736194,"A","CEC Survey",2017,15,"I",436.0360279216298,"TON",8,{"v":1.1276787972461002,"d":"1.13"},{"$f":"VLOOKUP(A13755,cordwood_density!A:D,4,FALSE)","v":1.1059},{"v":1.0196932790000002,"d":"1.02"}]
["20059","20","KS","059","Franklin","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",56.11945078296,"A","CEC Survey",2017,15,"I",27.510289878965793,"TON",8,{"$f":"P13763/J13763","v":{"v":0.49020953511039994,"d":"0.49"}},{"$f":"VLOOKUP(A13763,cordwood_density!A:D,4,FALSE)","v":1.2704},{"$f":"S13763/T13763","v":{"v":0.385870226,"d":"0.39"}}]
["20065","20","KS","065","Graham","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",11.49455703893488,"A","CEC Survey",2017,15,"I",32.85308970361361,"TON",8,{"v":2.8581431709227374,"d":"2.86"},{"$f":"VLOOKUP(A13802,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.19755741267318,"d":"2.20"}]
["20067","20","KS","067","Grant","","2104008620","Hydronic heater: indoor","Hydronic heater",4.904975429517591,"A","CEC Survey",2017,15,"I",13.614737014231954,"TON",8,{"v":2.7756993301740103,"d":"2.78"},{"$f":"VLOOKUP(A13820,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.13416833013533,"d":"2.13"}]
["20069","20","KS","069","Gray","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,332.894035864,"A","CEC Survey",2017,15,"I",83.63201997232478,"TON",8,{"v":0.251227150271,"d":"0.25"},{"$f":"VLOOKUP(A13841,cordwood_density!A:D,4,FALSE)","v":0.9962},{"v":0.252185455,"d":"0.25"}]
["20071","20","KS","071","Greeley","","2104009000","Wax Log; Total: All Combustor Types",null,7.924659258151474,"A","CEC Survey",2017,15,"I",1.1094522961412063,"TON",8,0.14,{"$f":"VLOOKUP(A13858,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.10764262648008613,"d":"0.11"}]
["20073","20","KS","073","Greenwood","","2104009000","Wax Log; Total: All Combustor Types",null,44.46792603966778,"A","CEC Survey",2017,15,"I",6.2255096455534895,"TON",8,0.14,{"$f":"VLOOKUP(A13873,cordwood_density!A:D,4,FALSE)","v":1.2636},{"v":0.11079455523899968,"d":"0.11"}]
["20077","20","KS","077","Harper","","2104008100","Fireplace: general","Fireplace: general",185.761288772,"A","CEC Survey",2017,15,"I",96.3487331426442,"TON",8,{"v":0.5186695989222,"d":"0.52"},{"$f":"VLOOKUP(A13897,cordwood_density!A:D,4,FALSE)","v":1.2078},{"v":0.429433349,"d":"0.43"}]
["20081","20","KS","081","Haskell","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",49.12513994849999,"A","CEC Survey",2017,15,"I",80.0493865621794,"TON",8,{"v":1.6294994099986,"d":"1.63"},{"$f":"VLOOKUP(A13936,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.252882831,"d":"1.25"}]
["20083","20","KS","083","Hodgeman","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",12.9260240352,"A","CEC Survey",2017,15,"I",20.709055557322404,"TON",8,{"v":1.6021210776746,"d":"1.60"},{"$f":"VLOOKUP(A13949,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.231832291,"d":"1.23"}]
["20087","20","KS","087","Jefferson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",166.477471692,"A","CEC Survey",2017,15,"I",88.46227766298534,"TON",8,{"v":0.5313768689775,"d":"0.53"},{"$f":"VLOOKUP(A13975,cordwood_density!A:D,4,FALSE)","v":1.2935},{"v":0.410805465,"d":"0.41"}]
["20089","20","KS","089","Jewell","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",67.4838926496,"A","CEC Survey",2017,15,"I",112.32049140631327,"TON",8,{"v":1.6644044526228,"d":"1.66"},{"$f":"VLOOKUP(A13996,cordwood_density!A:D,4,FALSE)","v":1.3041},{"v":1.276285908,"d":"1.28"}]
["20093","20","KS","093","Kearny","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",65.51135435304,"A","CEC Survey",2017,15,"I",106.59306196973068,"TON",8,{"v":1.6270929371312,"d":"1.63"},{"$f":"VLOOKUP(A14025,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.251032552,"d":"1.25"}]
["20095","20","KS","095","Kingman","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.5070306952643224,"A","CEC Survey",2017,15,"I",1.3329272614480234,"TON",8,{"v":2.628888692336761,"d":"2.63"},{"$f":"VLOOKUP(A14031,cordwood_density!A:D,4,FALSE)","v":1.2136},{"v":2.1661904188668104,"d":"2.17"}]
["20097","20","KS","097","Kiowa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",46.851045552,"A","CEC Survey",2017,15,"I",13.557838441337342,"TON",8,{"v":0.289381769,"d":"0.29"},{"$f":"VLOOKUP(A14052,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":0.3131837326839827,"d":"0.31"}]
["20101","20","KS","101","Lane","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",4.407189804,"A","CEC Survey",2017,15,"I",1.8978435189793834,"TON",8,{"v":0.4306244122404,"d":"0.43"},{"$f":"VLOOKUP(A14078,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.331096734,"d":"0.33"}]
["20105","20","KS","105","Lincoln","","2104009000","Wax Log; Total: All Combustor Types",null,20.453320959803904,"A","CEC Survey",2017,15,"I",2.863464934372547,"TON",8,0.14,{"$f":"VLOOKUP(A14113,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.10764262648008613,"d":"0.11"}]
["20107","20","KS","107","Linn","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",382.04114509561003,"A","CEC Survey",2017,15,"I",613.9373488936016,"TON",8,{"v":1.6069927461346,"d":"1.61"},{"$f":"VLOOKUP(A14130,cordwood_density!A:D,4,FALSE)","v":1.2263},{"v":1.310440142,"d":"1.31"}]
["20111","20","KS","111","Lyon","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",48.84457080070935,"A","CEC Survey",2017,15,"I",129.3888803727641,"TON",8,{"$f":"P14147/J14147","v":{"v":2.6489920630213635,"d":"2.65"}},{"$f":"VLOOKUP(A14147,cordwood_density!A:D,4,FALSE)","v":1.2185},{"$f":"S14147/T14147","v":{"v":2.1739778933289813,"d":"2.17"}}]
["20113","20","KS","113","McPherson","","2104008610","Hydronic heater: outdoor","Hydronic heater",58.714127243037616,"A","CEC Survey",2017,15,"I",151.7227703880254,"TON",8,{"v":2.584093088193129,"d":"2.58"},{"$f":"VLOOKUP(A14164,cordwood_density!A:D,4,FALSE)","v":1.2027},{"v":2.1485766094563306,"d":"2.15"}]
["20115","20","KS","115","Marion","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,754.556927925,"A","CEC Survey",2017,15,"I",227.46623784008062,"TON",8,{"v":0.30145669520999996,"d":"0.30"},{"$f":"VLOOKUP(A14186,cordwood_density!A:D,4,FALSE)","v":1.2045},{"v":0.25027538,"d":"0.25"}]
["20121","20","KS","121","Miami","","2104008620","Hydronic heater: indoor","Hydronic heater",53.1111613209396,"A","CEC Survey",2017,15,"I",162.22150672096444,"TON",8,{"v":3.054376946131792,"d":"3.05"},{"$f":"VLOOKUP(A14225,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":2.2579854706378297,"d":"2.26"}]
["20123","20","KS","123","Mitchell","","2104008620","Hydronic heater: indoor","Hydronic heater",10.142306943890734,"A","CEC Survey",2017,15,"I",25.88239194088835,"TON",8,{"v":2.5519235499452844,"d":"2.55"},{"$f":"VLOOKUP(A14240,cordwood_density!A:D,4,FALSE)","v":1.1634},{"v":2.1935048564081865,"d":"2.19"}]
["20125","20","KS","125","Montgomery","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",137.92468144704,"A","CEC Survey",2017,15,"I",187.1268024712853,"TON",8,{"v":1.3567318083176998,"d":"1.36"},{"$f":"VLOOKUP(A14264,cordwood_density!A:D,4,FALSE)","v":1.2283},{"v":1.104560619,"d":"1.10"}]
["20129","20","KS","129","Morton","","2104008620","Hydronic heater: indoor","Hydronic heater",4.836507506534897,"A","CEC Survey",2017,15,"I",13.494956187204162,"TON",8,{"v":2.7902274872871207,"d":"2.79"},{"$f":"VLOOKUP(A14285,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.145338680060834,"d":"2.15"}]
["20133","20","KS","133","Neosho","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8449951352629461,"A","CEC Survey",2017,15,"I",2.3382114910753593,"TON",8,{"v":2.7671301212257906,"d":"2.77"},{"$f":"VLOOKUP(A14316,cordwood_density!A:D,4,FALSE)","v":1.3118},{"v":2.1094146373119305,"d":"2.11"}]
["20133","20","KS","133","Neosho","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",108.35795324078322,"A","CEC Survey",2017,15,"I",53.65159878320671,"TON",8,{"v":0.49513300296460006,"d":"0.50"},{"$f":"VLOOKUP(A14320,cordwood_density!A:D,4,FALSE)","v":1.3118},{"v":0.377445497,"d":"0.38"}]
["20135","20","KS","135","Ness","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",59.96447254979999,"A","CEC Survey",2017,15,"I",74.54505425658114,"TON",8,{"v":1.2431536722794,"d":"1.24"},{"$f":"VLOOKUP(A14341,cordwood_density!A:D,4,FALSE)","v":0.9961},{"v":1.248020954,"d":"1.25"}]
["20139","20","KS","139","Osage","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",101.33629894752,"A","CEC Survey",2017,15,"I",150.15796450253677,"TON",8,{"v":1.4817786524875998,"d":"1.48"},{"$f":"VLOOKUP(A14369,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":1.2325558579999998,"d":"1.23"}]
["20143","20","KS","143","Ottawa","","2104009000","Wax Log; Total: All Combustor Types",null,39.09391621885656,"A","CEC Survey",2017,15,"I",5.4731482706399195,"TON",8,0.14,{"$f":"VLOOKUP(A14398,cordwood_density!A:D,4,FALSE)","v":1.1634},{"v":0.12033694344163659,"d":"0.12"}]
["20147","20","KS","147","Phillips","","2104008610","Hydronic heater: outdoor","Hydronic heater",15.07925043411236,"A","CEC Survey",2017,15,"I",43.73282599601487,"TON",8,{"v":2.900198931445706,"d":"2.90"},{"$f":"VLOOKUP(A14419,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2298930735396785,"d":"2.23"}]
["20149","20","KS","149","Pottawatomie","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",513.9774922257031,"A","CEC Survey",2017,15,"I",760.2001766586363,"TON",8,{"v":1.4790534374699997,"d":"1.48"},{"$f":"VLOOKUP(A14445,cordwood_density!A:D,4,FALSE)","v":1.239},{"v":1.1937477299999997,"d":"1.19"}]
["20151","20","KS","151","Pratt","","2104009000","Wax Log; Total: All Combustor Types",null,60.02849178947938,"A","CEC Survey",2017,15,"I",8.403988850527114,"TON",8,0.14,{"$f":"VLOOKUP(A14458,cordwood_density!A:D,4,FALSE)","v":1.2084},{"v":0.1158556769281695,"d":"0.12"}]
["20153","20","KS","153","Rawlins","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",89.61241518450001,"A","CEC Survey",2017,15,"I",146.5217349349904,"TON",8,{"v":1.6350606624464,"d":"1.64"},{"$f":"VLOOKUP(A14475,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.257158744,"d":"1.26"}]
["20159","20","KS","159","Rice","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",88.9601053196,"A","CEC Survey",2017,15,"I",30.839851556027593,"TON",8,{"v":0.346670582788,"d":"0.35"},{"$f":"VLOOKUP(A14514,cordwood_density!A:D,4,FALSE)","v":1.0004},{"v":0.34653197,"d":"0.35"}]
["20161","20","KS","161","Riley","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2382.444874502,"A","CEC Survey",2017,15,"I",771.1908232573475,"TON",8,{"$f":"P14531/J14531","v":{"v":0.32369723703200004,"d":"0.32"}},{"$f":"VLOOKUP(A14531,cordwood_density!A:D,4,FALSE)","v":1.3564},{"$f":"S14531/T14531","v":{"v":0.23864438000000002,"d":"0.24"}}]
["20165","20","KS","165","Rush","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.984398543767175,"A","CEC Survey",2017,15,"I",2.7779205827791533,"TON",8,{"v":2.821947066427369,"d":"2.82"},{"$f":"VLOOKUP(A14553,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.169727100128686,"d":"2.17"}]
["20167","20","KS","167","Russell","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",69.37342333263,"A","CEC Survey",2017,15,"I",28.94902805994764,"TON",8,{"v":0.41729277105359996,"d":"0.42"},{"$f":"VLOOKUP(A14574,cordwood_density!A:D,4,FALSE)","v":1.2168},{"v":0.3429427769999999,"d":"0.34"}]
["20171","20","KS","171","Scott","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",66.60642263,"A","CEC Survey",2017,15,"I",14.468923911548943,"TON",8,{"v":0.217230161,"d":"0.22"},{"$f":"VLOOKUP(A14607,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.16702303629094264,"d":"0.17"}]
["20171","20","KS","171","Scott","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",18.5987265738,"A","CEC Survey",2017,15,"I",25.089705570124444,"TON",8,{"v":1.3490012593371998,"d":"1.35"},{"$f":"VLOOKUP(A14609,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.037214562,"d":"1.04"}]
["20177","20","KS","177","Shawnee","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1898.394473919,"A","CEC Survey",2017,15,"I",524.7032817441105,"TON",8,{"v":0.276393178,"d":"0.28"},{"$f":"VLOOKUP(A14652,cordwood_density!A:D,4,FALSE)","v":1.2929},{"v":0.21377769201020963,"d":"0.21"}]
["20179","20","KS","179","Sheridan","","2104008620","Hydronic heater: indoor","Hydronic heater",7.034239593859155,"A","CEC Survey",2017,15,"I",20.017517061392844,"TON",8,{"v":2.84572579513328,"d":"2.85"},{"$f":"VLOOKUP(A14660,cordwood_density!A:D,4,FALSE)","v":1.2702},{"v":2.2403761574029915,"d":"2.24"}]
["20183","20","KS","183","Smith","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",16.69766417852906,"A","CEC Survey",2017,15,"I",39.937894075681406,"TON",8,{"v":2.3918252067277854,"d":"2.39"},{"$f":"VLOOKUP(A14687,cordwood_density!A:D,4,FALSE)","v":1.0693},{"v":2.2368139967528156,"d":"2.24"}]
["20185","20","KS","185","Stafford","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",10.022358540479999,"A","CEC Survey",2017,15,"I",4.642447207033238,"TON",8,{"v":0.46320905286740005,"d":"0.46"},{"$f":"VLOOKUP(A14708,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.35615027900000007,"d":"0.36"}]
["20189","20","KS","189","Stevens","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.18299336862529814,"A","CEC Survey",2017,15,"I",0.5084417756246367,"TON",8,{"v":2.77847104211593,"d":"2.78"},{"$f":"VLOOKUP(A14736,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.1362994326587192,"d":"2.14"}]
["20191","20","KS","191","Sumner","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",48.877802242299,"A","CEC Survey",2017,15,"I",124.7854647701379,"TON",8,{"v":2.5530089129528863,"d":"2.55"},{"$f":"VLOOKUP(A14747,cordwood_density!A:D,4,FALSE)","v":1.1928},{"v":2.140349524608389,"d":"2.14"}]
["20195","20","KS","195","Trego","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,233.775889464,"A","CEC Survey",2017,15,"I",54.43134471798577,"TON",8,{"v":0.23283557959200005,"d":"0.23"},{"$f":"VLOOKUP(A14786,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":0.251986558,"d":"0.25"}]
["20195","20","KS","195","Trego","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",21.5013041334,"A","CEC Survey",2017,15,"I",24.674577337809993,"TON",8,{"v":1.1475851504040002,"d":"1.15"},{"$f":"VLOOKUP(A14789,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":1.2419752710000003,"d":"1.24"}]
["20201","20","KS","201","Washington","","2104008620","Hydronic heater: indoor","Hydronic heater",15.125061687454098,"A","CEC Survey",2017,15,"I",45.92461497604045,"TON",8,{"v":3.0363257965508925,"d":"3.04"},{"$f":"VLOOKUP(A14825,cordwood_density!A:D,4,FALSE)","v":1.3621},{"v":2.2291504269516866,"d":"2.23"}]
["20203","20","KS","203","Wichita","","2104008100","Fireplace: general","Fireplace: general",72.23270082,"A","CEC Survey",2017,15,"I",40.26882035665909,"TON",8,{"v":0.5574873969756,"d":"0.56"},{"$f":"VLOOKUP(A14842,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.428638626,"d":"0.43"}]
["20205","20","KS","205","Wilson","","2104008610","Hydronic heater: outdoor","Hydronic heater",22.806475246009875,"A","CEC Survey",2017,15,"I",58.17907239071782,"TON",8,{"v":2.550989215262301,"d":"2.55"},{"$f":"VLOOKUP(A14854,cordwood_density!A:D,4,FALSE)","v":1.1907},{"v":2.1424281643254393,"d":"2.14"}]
["20207","20","KS","207","Woodson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",73.10592796569999,"A","CEC Survey",2017,15,"I",112.35148278731585,"TON",8,{"v":1.5368313611999997,"d":"1.54"},{"$f":"VLOOKUP(A14881,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":1.2393801299999998,"d":"1.24"}]
["21003","21","KY","003","Allen","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",183.61262916080003,"A","CEC Survey",2017,15,"I",179.05630376001025,"TON",8,{"v":0.9751851197730003,"d":"0.98"},{"$f":"VLOOKUP(A14920,cordwood_density!A:D,4,FALSE)","v":1.431},{"v":0.6814710830000001,"d":"0.68"}]
["21005","21","KY","005","Anderson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",318.51647516304,"A","CEC Survey",2017,15,"I",664.7980042470258,"TON",8,{"v":2.0871699145444,"d":"2.09"},{"$f":"VLOOKUP(A14941,cordwood_density!A:D,4,FALSE)","v":1.3762},{"v":1.5166181619999999,"d":"1.52"}]
["21007","21","KY","007","Ballard","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,494.04149099999995,"A","CEC Survey",2017,15,"I",207.85178422012183,"TON",8,{"v":0.420717263644,"d":"0.42"},{"$f":"VLOOKUP(A14951,cordwood_density!A:D,4,FALSE)","v":1.292},{"v":0.325632557,"d":"0.33"}]
["21011","21","KY","011","Bath","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.108605261788684,"A","CEC Survey",2017,15,"I",4.888400684108433,"TON",8,{"v":4.409505215789092,"d":"4.41"},{"$f":"VLOOKUP(A14976,cordwood_density!A:D,4,FALSE)","v":1.4451},{"v":3.051349536910312,"d":"3.05"}]
["21013","21","KY","013","Bell","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",346.054998822,"A","CEC Survey",2017,15,"I",400.9591620064167,"TON",8,{"v":1.158657333,"d":"1.16"},{"$f":"VLOOKUP(A14997,cordwood_density!A:D,4,FALSE)","v":1.3363},{"v":0.8670637828331962,"d":"0.87"}]
["21017","21","KY","017","Bourbon","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",277.595313824,"A","CEC Survey",2017,15,"I",111.26991622866649,"TON",8,{"v":0.400834995,"d":"0.40"},{"$f":"VLOOKUP(A15027,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.33341789635667946,"d":"0.33"}]
["21019","21","KY","019","Boyd","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.640372886985533,"A","CEC Survey",2017,15,"I",10.135759507385542,"TON",8,{"v":3.8387606376905947,"d":"3.84"},{"$f":"VLOOKUP(A15036,cordwood_density!A:D,4,FALSE)","v":1.396},{"v":2.7498285370276467,"d":"2.75"}]
["21023","21","KY","023","Bracken","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",224.05075082473996,"A","CEC Survey",2017,15,"I",486.4295610068832,"TON",8,{"v":2.1710686494748,"d":"2.17"},{"$f":"VLOOKUP(A15075,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":1.8059130340000003,"d":"1.81"}]
["21025","21","KY","025","Breathitt","","2104008620","Hydronic heater: indoor","Hydronic heater",31.85130850388919,"A","CEC Survey",2017,15,"I",135.14339038488922,"TON",8,{"v":4.242946262894901,"d":"4.24"},{"$f":"VLOOKUP(A15080,cordwood_density!A:D,4,FALSE)","v":1.3536},{"v":3.134564319514555,"d":"3.13"}]
["21029","21","KY","029","Bullitt","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",813.1929291488799,"A","CEC Survey",2017,15,"I",899.8629591308691,"TON",8,{"v":1.1065799109599999,"d":"1.11"},{"$f":"VLOOKUP(A15114,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.8924031539999999,"d":"0.89"}]
["21031","21","KY","031","Butler","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,798.2177172199999,"A","CEC Survey",2017,15,"I",327.8732449568898,"TON",8,{"v":0.41075666185259996,"d":"0.41"},{"$f":"VLOOKUP(A15131,cordwood_density!A:D,4,FALSE)","v":1.2642},{"v":0.32491430299999996,"d":"0.32"}]
["21035","21","KY","035","Calloway","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.9338243483416038,"A","CEC Survey",2017,15,"I",7.732202031707904,"TON",8,{"v":3.998399357386742,"d":"4.00"},{"$f":"VLOOKUP(A15156,cordwood_density!A:D,4,FALSE)","v":1.4506},{"v":2.7563762287237985,"d":"2.76"}]
["21037","21","KY","037","Campbell","","2104008620","Hydronic heater: indoor","Hydronic heater",80.09499572909026,"A","CEC Survey",2017,15,"I",262.4180212837092,"TON",8,{"v":3.276334793390841,"d":"3.28"},{"$f":"VLOOKUP(A15170,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":2.5386136629403695,"d":"2.54"}]
["21041","21","KY","041","Carroll","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",134.3945897539,"A","CEC Survey",2017,15,"I",312.1235555838589,"TON",8,{"v":2.3224413732383997,"d":"2.32"},{"$f":"VLOOKUP(A15209,cordwood_density!A:D,4,FALSE)","v":1.4389},{"v":1.6140394559999998,"d":"1.61"}]
["21043","21","KY","043","Carter","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1556.5848377200002,"A","CEC Survey",2017,15,"I",683.0665852578993,"TON",8,{"v":0.43882387179,"d":"0.44"},{"$f":"VLOOKUP(A15221,cordwood_density!A:D,4,FALSE)","v":1.3425},{"v":0.326870668,"d":"0.33"}]
["21047","21","KY","047","Christian","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",411.2000471655,"A","CEC Survey",2017,15,"I",375.4328672788573,"TON",8,{"v":0.9130175686184999,"d":"0.91"},{"$f":"VLOOKUP(A15248,cordwood_density!A:D,4,FALSE)","v":1.4071},{"v":0.648864735,"d":"0.65"}]
["21049","21","KY","049","Clark","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",218.02151748160003,"A","CEC Survey",2017,15,"I",156.77309029456057,"TON",8,{"v":0.7190716407512,"d":"0.72"},{"$f":"VLOOKUP(A15265,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.598129796,"d":"0.60"}]
["21053","21","KY","053","Clinton","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",153.57934493684365,"A","CEC Survey",2017,15,"I",144.037784134756,"TON",8,{"v":0.9378721089999998,"d":"0.94"},{"$f":"VLOOKUP(A15297,cordwood_density!A:D,4,FALSE)","v":1.4499},{"v":0.6468529615835574,"d":"0.65"}]
["21055","21","KY","055","Crittenden","","2104008610","Hydronic heater: outdoor","Hydronic heater",27.04401093815174,"A","CEC Survey",2017,15,"I",99.43159245252183,"TON",8,{"v":3.6766584912244253,"d":"3.68"},{"$f":"VLOOKUP(A15304,cordwood_density!A:D,4,FALSE)","v":1.2614},{"v":2.91474432473793,"d":"2.91"}]
["21057","21","KY","057","Cumberland","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",79.3408582512,"A","CEC Survey",2017,15,"I",113.4663292618542,"TON",8,{"v":1.4301121989708003,"d":"1.43"},{"$f":"VLOOKUP(A15325,cordwood_density!A:D,4,FALSE)","v":1.4191},{"v":1.007759988,"d":"1.01"}]
["21063","21","KY","063","Elliott","","2104008610","Hydronic heater: outdoor","Hydronic heater",28.13753423237031,"A","CEC Survey",2017,15,"I",123.27931638477199,"TON",8,{"v":4.381312000073821,"d":"4.38"},{"$f":"VLOOKUP(A15364,cordwood_density!A:D,4,FALSE)","v":1.3706},{"v":3.1966379688266606,"d":"3.20"}]
["21063","21","KY","063","Elliott","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,375.15177215737253,"A","CEC Survey",2017,15,"I",167.85585070831482,"TON",8,{"v":0.4474345136184001,"d":"0.45"},{"$f":"VLOOKUP(A15371,cordwood_density!A:D,4,FALSE)","v":1.3706},{"v":0.326451564,"d":"0.33"}]
["21067","21","KY","067","Fayette","","2104009000","Wax Log; Total: All Combustor Types",null,1828.9234250863562,"A","CEC Survey",2017,15,"I",256.0492795120899,"TON",8,{"v":0.14000000000000004,"d":"0.14"},{"$f":"VLOOKUP(A15403,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.11645316918981871,"d":"0.12"}]
["21069","21","KY","069","Fleming","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",375.56877899052,"A","CEC Survey",2017,15,"I",893.2735421317161,"TON",8,{"v":2.378455271316,"d":"2.38"},{"$f":"VLOOKUP(A15420,cordwood_density!A:D,4,FALSE)","v":1.396},{"v":1.703764521,"d":"1.70"}]
["21073","21","KY","073","Franklin","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",554.6487185039999,"A","CEC Survey",2017,15,"I",294.3144270190068,"TON",8,{"v":0.530632123,"d":"0.53"},{"$f":"VLOOKUP(A15447,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.4111514977529831,"d":"0.41"}]
["21075","21","KY","075","Fulton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",52.09172508983999,"A","CEC Survey",2017,15,"I",32.724297412103304,"TON",8,{"v":0.628205292792,"d":"0.63"},{"$f":"VLOOKUP(A15459,cordwood_density!A:D,4,FALSE)","v":1.148},{"v":0.547217154,"d":"0.55"}]
["21081","21","KY","081","Grant","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.155793349416059,"A","CEC Survey",2017,15,"I",18.525563334004985,"TON",8,{"v":3.593154744284539,"d":"3.59"},{"$f":"VLOOKUP(A15498,cordwood_density!A:D,4,FALSE)","v":1.2139},{"v":2.960008851045835,"d":"2.96"}]
["21083","21","KY","083","Graves","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",83.66237188091651,"A","CEC Survey",2017,15,"I",332.2224479078722,"TON",8,{"v":3.9709900692362816,"d":"3.97"},{"$f":"VLOOKUP(A15512,cordwood_density!A:D,4,FALSE)","v":1.4245},{"v":2.787637816241686,"d":"2.79"}]
["21085","21","KY","085","Grayson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",354.348998172,"A","CEC Survey",2017,15,"I",257.30771609808926,"TON",8,{"v":0.7261420729999999,"d":"0.73"},{"$f":"VLOOKUP(A15537,cordwood_density!A:D,4,FALSE)","v":1.3332},{"v":0.5446610208520851,"d":"0.54"}]
["21087","21","KY","087","Green","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",228.99571064025002,"A","CEC Survey",2017,15,"I",557.9078402329455,"TON",8,{"v":2.4363244126848,"d":"2.44"},{"$f":"VLOOKUP(A15554,cordwood_density!A:D,4,FALSE)","v":1.4303},{"v":1.7033660160000001,"d":"1.70"}]
["21093","21","KY","093","Hardin","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.933797252400796,"A","CEC Survey",2017,15,"I",58.38372387808306,"TON",8,{"v":3.9095029141832724,"d":"3.91"},{"$f":"VLOOKUP(A15588,cordwood_density!A:D,4,FALSE)","v":1.3716},{"v":2.8503229178938994,"d":"2.85"}]
["21093","21","KY","093","Hardin","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",809.7390653310799,"A","CEC Survey",2017,15,"I",789.1035535286751,"TON",8,{"v":0.9745158499992,"d":"0.97"},{"$f":"VLOOKUP(A15593,cordwood_density!A:D,4,FALSE)","v":1.3716},{"v":0.710495662,"d":"0.71"}]
["21099","21","KY","099","Hart","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",61.39580208573224,"A","CEC Survey",2017,15,"I",244.9214126415417,"TON",8,{"v":3.9892208314102136,"d":"3.99"},{"$f":"VLOOKUP(A15632,cordwood_density!A:D,4,FALSE)","v":1.3523},{"v":2.9499525485544726,"d":"2.95"}]
["21099","21","KY","099","Hart","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1123.8054561220001,"A","CEC Survey",2017,15,"I",495.78816225243014,"TON",8,{"v":0.4411690293472,"d":"0.44"},{"$f":"VLOOKUP(A15641,cordwood_density!A:D,4,FALSE)","v":1.3523},{"v":0.326236064,"d":"0.33"}]
["21103","21","KY","103","Henry","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1006.247629016,"A","CEC Survey",2017,15,"I",383.39625101912367,"TON",8,{"v":0.3810158056164,"d":"0.38"},{"$f":"VLOOKUP(A15671,cordwood_density!A:D,4,FALSE)","v":1.1652},{"v":0.326996057,"d":"0.33"}]
["21107","21","KY","107","Hopkins","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",100.19908867858125,"A","CEC Survey",2017,15,"I",351.3028873025523,"TON",8,{"v":3.506048726944634,"d":"3.51"},{"$f":"VLOOKUP(A15692,cordwood_density!A:D,4,FALSE)","v":1.2687},{"v":2.7634970654564786,"d":"2.76"}]
["21109","21","KY","109","Jackson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",227.07511525,"A","CEC Survey",2017,15,"I",281.00001281258784,"TON",8,{"v":1.237476033,"d":"1.24"},{"$f":"VLOOKUP(A15717,cordwood_density!A:D,4,FALSE)","v":1.4435},{"v":0.8572747024593004,"d":"0.86"}]
["21111","21","KY","111","Jefferson","","2104008100","Fireplace: general","Fireplace: general",39773.034923904,"A","CEC Survey",2017,15,"I",11325.276239934214,"TON",8,{"v":0.28474760001599997,"d":"0.28"},{"$f":"VLOOKUP(A15727,cordwood_density!A:D,4,FALSE)","v":1.348},{"v":0.21123709199999996,"d":"0.21"}]
["21113","21","KY","113","Jessamine","","2104009000","Wax Log; Total: All Combustor Types",null,266.2464152386268,"A","CEC Survey",2017,15,"I",37.274498133407754,"TON",8,0.14,{"$f":"VLOOKUP(A15748,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.11645316918981868,"d":"0.12"}]
["21119","21","KY","119","Knott","","2104008100","Fireplace: general","Fireplace: general",822.042270396,"A","CEC Survey",2017,15,"I",368.9044299806823,"TON",8,{"v":0.448765767,"d":"0.45"},{"$f":"VLOOKUP(A15787,cordwood_density!A:D,4,FALSE)","v":1},{"v":0.448765767,"d":"0.45"}]
["21121","21","KY","121","Knox","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",325.49607894888,"A","CEC Survey",2017,15,"I",441.67419459622596,"TON",8,{"v":1.3569263138976002,"d":"1.36"},{"$f":"VLOOKUP(A15803,cordwood_density!A:D,4,FALSE)","v":1.2956},{"v":1.047334296,"d":"1.05"}]
["21123","21","KY","123","Larue","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",228.46740121800002,"A","CEC Survey",2017,15,"I",445.84944725850545,"TON",8,{"v":1.9514794884592,"d":"1.95"},{"$f":"VLOOKUP(A15826,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":1.623256936,"d":"1.62"}]
["21127","21","KY","127","Lawrence","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.608691536589992,"A","CEC Survey",2017,15,"I",16.641001149566495,"TON",8,{"v":3.6107864927491558,"d":"3.61"},{"$f":"VLOOKUP(A15843,cordwood_density!A:D,4,FALSE)","v":1.1655},{"v":3.0980579088366844,"d":"3.10"}]
["21131","21","KY","131","Leslie","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",209.70890487111998,"A","CEC Survey",2017,15,"I",341.31414506433975,"TON",8,{"v":1.6275615252203997,"d":"1.63"},{"$f":"VLOOKUP(A15879,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":1.172510284,"d":"1.17"}]
["21131","21","KY","131","Leslie","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",157.5240183,"A","CEC Survey",2017,15,"I",231.29856577981278,"TON",8,{"v":1.468338405,"d":"1.47"},{"$f":"VLOOKUP(A15882,cordwood_density!A:D,4,FALSE)","v":1.3881},{"v":1.0578044845472228,"d":"1.06"}]
["21137","21","KY","137","Lincoln","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.284789530367814,"A","CEC Survey",2017,15,"I",10.275714579006097,"TON",8,{"v":4.497444706581737,"d":"4.50"},{"$f":"VLOOKUP(A15921,cordwood_density!A:D,4,FALSE)","v":1.4977},{"v":3.002900919130491,"d":"3.00"}]
["21139","21","KY","139","Livingston","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",36.42242593252753,"A","CEC Survey",2017,15,"I",156.77624975283175,"TON",8,{"v":4.304387907693448,"d":"4.30"},{"$f":"VLOOKUP(A15932,cordwood_density!A:D,4,FALSE)","v":1.4635},{"v":2.9411601692473166,"d":"2.94"}]
["21141","21","KY","141","Logan","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",560.285825253,"A","CEC Survey",2017,15,"I",1211.2391365757887,"TON",8,{"v":2.1618236299817997,"d":"2.16"},{"$f":"VLOOKUP(A15960,cordwood_density!A:D,4,FALSE)","v":1.3638},{"v":1.585147111,"d":"1.59"}]
["21145","21","KY","145","McCracken","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.5510059974436365,"A","CEC Survey",2017,15,"I",9.923518971800483,"TON",8,{"v":3.8900414117978723,"d":"3.89"},{"$f":"VLOOKUP(A15981,cordwood_density!A:D,4,FALSE)","v":1.4559},{"v":2.671915249534908,"d":"2.67"}]
["21149","21","KY","149","Mclean","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.3870556479523453,"A","CEC Survey",2017,15,"I",8.275621053474511,"TON",8,{"v":3.4668739543518696,"d":"3.47"},{"$f":"VLOOKUP(A16008,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":2.883774708327957,"d":"2.88"}]
["21149","21","KY","149","Mclean","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,588.33394847,"A","CEC Survey",2017,15,"I",230.68877650476657,"TON",8,{"v":0.3921051591612,"d":"0.39"},{"$f":"VLOOKUP(A16016,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.326156346,"d":"0.33"}]
["21153","21","KY","153","Magoffin","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",50.233542001755936,"A","CEC Survey",2017,15,"I",194.1183104085666,"TON",8,{"v":3.8643166034714636,"d":"3.86"},{"$f":"VLOOKUP(A16037,cordwood_density!A:D,4,FALSE)","v":1.2179},{"v":3.172934233903821,"d":"3.17"}]
["21155","21","KY","155","Marion","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1129.997404125,"A","CEC Survey",2017,15,"I",491.6143571429571,"TON",8,{"v":0.43505795265399994,"d":"0.44"},{"$f":"VLOOKUP(A16061,cordwood_density!A:D,4,FALSE)","v":1.339},{"v":0.32491258599999995,"d":"0.32"}]
["21161","21","KY","161","Mason","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.184241578966155,"A","CEC Survey",2017,15,"I",12.509218607619536,"TON",8,{"v":3.9284766238373696,"d":"3.93"},{"$f":"VLOOKUP(A16098,cordwood_density!A:D,4,FALSE)","v":1.3752},{"v":2.8566583942970984,"d":"2.86"}]
["21163","21","KY","163","Meade","","2104008620","Hydronic heater: indoor","Hydronic heater",53.00578509255103,"A","CEC Survey",2017,15,"I",223.69902643370312,"TON",8,{"v":4.220275693362757,"d":"4.22"},{"$f":"VLOOKUP(A16115,cordwood_density!A:D,4,FALSE)","v":1.4332},{"v":2.9446523118634924,"d":"2.94"}]
["21165","21","KY","165","Menifee","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",117.88167963,"A","CEC Survey",2017,15,"I",138.71657642524994,"TON",8,{"v":1.176744146,"d":"1.18"},{"$f":"VLOOKUP(A16137,cordwood_density!A:D,4,FALSE)","v":1.4204},{"v":0.8284596916361588,"d":"0.83"}]
["21167","21","KY","167","Mercer","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",326.4836223362344,"A","CEC Survey",2017,15,"I",594.5764903065119,"TON",8,{"v":1.8211525774305999,"d":"1.82"},{"$f":"VLOOKUP(A16154,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":1.5148499229999999,"d":"1.51"}]
["21169","21","KY","169","Metcalfe","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",168.9392788664,"A","CEC Survey",2017,15,"I",412.844245026077,"TON",8,{"v":2.4437433839916003,"d":"2.44"},{"$f":"VLOOKUP(A16171,cordwood_density!A:D,4,FALSE)","v":1.4086},{"v":1.734873906,"d":"1.73"}]
["21175","21","KY","175","Morgan","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",148.37903055864,"A","CEC Survey",2017,15,"I",206.5201076725674,"TON",8,{"v":1.3918416025164,"d":"1.39"},{"$f":"VLOOKUP(A16210,cordwood_density!A:D,4,FALSE)","v":1.3146},{"v":1.058756734,"d":"1.06"}]
["21177","21","KY","177","Muhlenberg","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",259.93522826663997,"A","CEC Survey",2017,15,"I",238.25492564654917,"TON",8,{"v":0.9165934422792001,"d":"0.92"},{"$f":"VLOOKUP(A16223,cordwood_density!A:D,4,FALSE)","v":1.2516},{"v":0.7323373620000001,"d":"0.73"}]
["21181","21","KY","181","Nicholas","","2104008610","Hydronic heater: outdoor","Hydronic heater",23.656080318679052,"A","CEC Survey",2017,15,"I",91.54402458621946,"TON",8,{"v":3.869788373771097,"d":"3.87"},{"$f":"VLOOKUP(A16249,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":2.998441324787771,"d":"3.00"}]
["21183","21","KY","183","Ohio","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",202.3289741046,"A","CEC Survey",2017,15,"I",206.65276609986608,"TON",8,{"v":1.0213701078375002,"d":"1.02"},{"$f":"VLOOKUP(A16270,cordwood_density!A:D,4,FALSE)","v":1.3415},{"v":0.7613642250000001,"d":"0.76"}]
["21187","21","KY","187","Owen","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",148.59605384256,"A","CEC Survey",2017,15,"I",172.10828928561887,"TON",8,{"v":1.158229204848,"d":"1.16"},{"$f":"VLOOKUP(A16299,cordwood_density!A:D,4,FALSE)","v":1.5208},{"v":0.7615920600000001,"d":"0.76"}]
["21187","21","KY","187","Owen","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",293.78133372431995,"A","CEC Survey",2017,15,"I",811.5362286119804,"TON",8,{"v":2.7623818651920002,"d":"2.76"},{"$f":"VLOOKUP(A16305,cordwood_density!A:D,4,FALSE)","v":1.5208},{"v":1.8164004900000001,"d":"1.82"}]
["21193","21","KY","193","Perry","","2104009000","Wax Log; Total: All Combustor Types",null,158.5241239137252,"A","CEC Survey",2017,15,"I",22.19337734792153,"TON",8,0.14,{"$f":"VLOOKUP(A16348,cordwood_density!A:D,4,FALSE)","v":1.3437},{"v":0.10418992334598498,"d":"0.10"}]
["21195","21","KY","195","Pike","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",255.30547305767033,"A","CEC Survey",2017,15,"I",1001.5582589036112,"TON",8,{"v":3.9229799773127922,"d":"3.92"},{"$f":"VLOOKUP(A16352,cordwood_density!A:D,4,FALSE)","v":1.2663},{"v":3.0979862412641492,"d":"3.10"}]
["21199","21","KY","199","Pulaski","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.512615017386777,"A","CEC Survey",2017,15,"I",60.9213116762724,"TON",8,{"v":4.197817664375847,"d":"4.20"},{"$f":"VLOOKUP(A16383,cordwood_density!A:D,4,FALSE)","v":1.4138},{"v":2.969173620296964,"d":"2.97"}]
["21201","21","KY","201","Robertson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",33.99924908898,"A","CEC Survey",2017,15,"I",36.26497377800231,"TON",8,{"v":1.066640433237,"d":"1.07"},{"$f":"VLOOKUP(A16404,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8264686450000001,"d":"0.83"}]
["21205","21","KY","205","Rowan","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.94664108198646,"A","CEC Survey",2017,15,"I",25.893143663031086,"TON",8,{"v":4.354246927978634,"d":"4.35"},{"$f":"VLOOKUP(A16428,cordwood_density!A:D,4,FALSE)","v":1.4701},{"v":2.9618712522812287,"d":"2.96"}]
["21207","21","KY","207","Russell","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.605160465171169,"A","CEC Survey",2017,15,"I",21.87996919598869,"TON",8,{"v":3.903540198705181,"d":"3.90"},{"$f":"VLOOKUP(A16443,cordwood_density!A:D,4,FALSE)","v":1.2908},{"v":3.0241247278472123,"d":"3.02"}]
["21211","21","KY","211","Shelby","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",580.2887761679999,"A","CEC Survey",2017,15,"I",285.7625120576889,"TON",8,{"v":0.492448801,"d":"0.49"},{"$f":"VLOOKUP(A16482,cordwood_density!A:D,4,FALSE)","v":1.348},{"v":0.3653181016320474,"d":"0.37"}]
["21215","21","KY","215","Spencer","","2104008610","Hydronic heater: outdoor","Hydronic heater",74.43922617201605,"A","CEC Survey",2017,15,"I",306.73838294690705,"TON",8,{"v":4.120655180349245,"d":"4.12"},{"$f":"VLOOKUP(A16504,cordwood_density!A:D,4,FALSE)","v":1.379},{"v":2.988147338904456,"d":"2.99"}]
["21217","21","KY","217","Taylor","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.4936937256293832,"A","CEC Survey",2017,15,"I",5.779131879562169,"TON",8,{"v":3.8690206569135,"d":"3.87"},{"$f":"VLOOKUP(A16521,cordwood_density!A:D,4,FALSE)","v":1.3783},{"v":2.807096174209896,"d":"2.81"}]
["21219","21","KY","219","Todd","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",106.1016488044,"A","CEC Survey",2017,15,"I",89.07339717767582,"TON",8,{"v":0.8395100187545999,"d":"0.84"},{"$f":"VLOOKUP(A16538,cordwood_density!A:D,4,FALSE)","v":1.4557},{"v":0.5767053779999999,"d":"0.58"}]
["21223","21","KY","223","Trimble","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",132.35859519417,"A","CEC Survey",2017,15,"I",117.96477090866222,"TON",8,{"v":0.8912513066159999,"d":"0.89"},{"$f":"VLOOKUP(A16569,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.74135028,"d":"0.74"}]
["21225","21","KY","225","Union","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",32.14990628876123,"A","CEC Survey",2017,15,"I",109.12041606298172,"TON",8,{"v":3.3941130366879912,"d":"3.39"},{"$f":"VLOOKUP(A16577,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":2.8232515693628275,"d":"2.82"}]
["21229","21","KY","229","Washington","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,725.8978707,"A","CEC Survey",2017,15,"I",279.89492890614116,"TON",8,{"v":0.3855844467986,"d":"0.39"},{"$f":"VLOOKUP(A16616,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.320732363,"d":"0.32"}]
["21233","21","KY","233","Webster","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",39.74978632602769,"A","CEC Survey",2017,15,"I",137.30938254160685,"TON",8,{"v":3.454342657728912,"d":"3.45"},{"$f":"VLOOKUP(A16637,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":2.8733510711436634,"d":"2.87"}]
["21233","21","KY","233","Webster","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",106.23668001955,"A","CEC Survey",2017,15,"I",77.01772856499805,"TON",8,{"$f":"P16643/J16643","v":{"v":0.7249636241533999,"d":"0.72"}},{"$f":"VLOOKUP(A16643,cordwood_density!A:D,4,FALSE)","v":1.2022},{"$f":"S16643/T16643","v":{"v":0.603030797,"d":"0.60"}}]
["21237","21","KY","237","Wolfe","","2104008100","Fireplace: general","Fireplace: general",337.519517463,"A","CEC Survey",2017,15,"I",217.2778452346064,"TON",8,{"v":0.643748980408,"d":"0.64"},{"$f":"VLOOKUP(A16672,cordwood_density!A:D,4,FALSE)","v":1.4255},{"v":0.451595216,"d":"0.45"}]
["21239","21","KY","239","Woodford","","2104009000","Wax Log; Total: All Combustor Types",null,144.53458901366466,"A","CEC Survey",2017,15,"I",20.234842461913054,"TON",8,0.14,{"$f":"VLOOKUP(A16693,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.10847667751433443,"d":"0.11"}]
["22003","22","LA","003","Allen","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",296.52362204203996,"A","CEC Survey",2017,15,"I",99.14778684859475,"TON",8,{"v":0.3343672459071,"d":"0.33"},{"$f":"VLOOKUP(A16719,cordwood_density!A:D,4,FALSE)","v":1.3007},{"v":0.257067153,"d":"0.26"}]
["22005","22","LA","005","Ascension","","2104008100","Fireplace: general","Fireplace: general",4755.80066322,"A","CEC Survey",2017,15,"I",538.4766437617794,"TON",8,{"v":0.11322523417060001,"d":"0.11"},{"$f":"VLOOKUP(A16732,cordwood_density!A:D,4,FALSE)","v":1.1549},{"v":0.098038994,"d":"0.10"}]
["22009","22","LA","009","Avoyelles","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",373.66301202216005,"A","CEC Survey",2017,15,"I",197.90351147392434,"TON",8,{"$f":"P16771/J16771","v":{"v":0.5296309913119999,"d":"0.53"}},{"$f":"VLOOKUP(A16771,cordwood_density!A:D,4,FALSE)","v":1.388},{"$f":"S16771/T16771","v":{"v":0.3815785239999999,"d":"0.38"}}]
["22013","22","LA","013","Bienville","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",146.4601235802788,"A","CEC Survey",2017,15,"I",51.8891722568319,"TON",8,{"v":0.3542887373599,"d":"0.35"},{"$f":"VLOOKUP(A16795,cordwood_density!A:D,4,FALSE)","v":1.3097},{"v":0.270511367,"d":"0.27"}]
["22015","22","LA","015","Bossier","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",894.47039538752,"A","CEC Survey",2017,15,"I",296.659202820645,"TON",8,{"v":0.3316590513788,"d":"0.33"},{"$f":"VLOOKUP(A16810,cordwood_density!A:D,4,FALSE)","v":1.3892},{"v":0.238741039,"d":"0.24"}]
["22017","22","LA","017","Caddo","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2426.766461256,"A","CEC Survey",2017,15,"I",190.32857315110505,"TON",8,{"v":0.078428879,"d":"0.08"},{"$f":"VLOOKUP(A16827,cordwood_density!A:D,4,FALSE)","v":1.3066},{"v":0.06002516378386653,"d":"0.06"}]
["22021","22","LA","021","Caldwell","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",211.37486223679997,"A","CEC Survey",2017,15,"I",132.42050660059417,"TON",8,{"v":0.6264723496412999,"d":"0.63"},{"$f":"VLOOKUP(A16860,cordwood_density!A:D,4,FALSE)","v":1.3857},{"v":0.45209810899999997,"d":"0.45"}]
["22023","22","LA","023","Cameron","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.20277602285054014,"A","CEC Survey",2017,15,"I",0.175787302545797,"TON",8,{"v":0.8669037890903123,"d":"0.87"},{"$f":"VLOOKUP(A16866,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.6717060197507456,"d":"0.67"}]
["22027","22","LA","027","Claiborne","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",282.19564104939997,"A","CEC Survey",2017,15,"I",156.54883516826285,"TON",8,{"v":0.5547528465929,"d":"0.55"},{"$f":"VLOOKUP(A16905,cordwood_density!A:D,4,FALSE)","v":1.2679},{"v":0.437536751,"d":"0.44"}]
["22029","22","LA","029","Concordia","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",142.38675948726197,"A","CEC Survey",2017,15,"I",28.523433442406937,"TON",8,{"v":0.20032363644710002,"d":"0.20"},{"$f":"VLOOKUP(A16913,cordwood_density!A:D,4,FALSE)","v":1.2049},{"v":0.166257479,"d":"0.17"}]
["22033","22","LA","033","East Baton Rouge","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3701.5507512908393,"A","CEC Survey",2017,15,"I",967.4787407742705,"TON",8,{"v":0.26137119433979994,"d":"0.26"},{"$f":"VLOOKUP(A16944,cordwood_density!A:D,4,FALSE)","v":1.2326},{"v":0.21204867299999997,"d":"0.21"}]
["22035","22","LA","035","East Carroll","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,321.57626673,"A","CEC Survey",2017,15,"I",29.526889400103446,"TON",8,{"v":0.091819243069,"d":"0.09"},{"$f":"VLOOKUP(A16961,cordwood_density!A:D,4,FALSE)","v":1.1294},{"v":0.081299135,"d":"0.08"}]
["22039","22","LA","039","Evangeline","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",377.05159189656,"A","CEC Survey",2017,15,"I",95.39787275980292,"TON",8,{"v":0.253010131266,"d":"0.25"},{"$f":"VLOOKUP(A16989,cordwood_density!A:D,4,FALSE)","v":1.2954},{"v":0.19531429,"d":"0.20"}]
["22041","22","LA","041","Franklin","","2104008620","Hydronic heater: indoor","Hydronic heater",17.350236495711815,"A","CEC Survey",2017,15,"I",14.947508203501464,"TON",8,{"v":0.8615161071260212,"d":"0.86"},{"$f":"VLOOKUP(A17000,cordwood_density!A:D,4,FALSE)","v":1.2808},{"v":0.672639059280154,"d":"0.67"}]
["22043","22","LA","043","Grant","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1184.992839162,"A","CEC Survey",2017,15,"I",125.0327924089787,"TON",8,{"v":0.1055135425944,"d":"0.11"},{"$f":"VLOOKUP(A17021,cordwood_density!A:D,4,FALSE)","v":1.2536},{"v":0.084168429,"d":"0.08"}]
["22049","22","LA","049","Jackson","","2104008620","Hydronic heater: indoor","Hydronic heater",20.947579659299848,"A","CEC Survey",2017,15,"I",19.198288703107853,"TON",8,{"v":0.9164919773719356,"d":"0.92"},{"$f":"VLOOKUP(A17060,cordwood_density!A:D,4,FALSE)","v":1.3833},{"v":0.6625402858179249,"d":"0.66"}]
["22049","22","LA","049","Jackson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",173.57672457008002,"A","CEC Survey",2017,15,"I",69.86960074438939,"TON",8,{"v":0.4025286277145999,"d":"0.40"},{"$f":"VLOOKUP(A17063,cordwood_density!A:D,4,FALSE)","v":1.3833},{"v":0.2909915619999999,"d":"0.29"}]
["22053","22","LA","053","Jefferson Davis","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",289.79797103065,"A","CEC Survey",2017,15,"I",114.4474932182719,"TON",8,{"v":0.39492165114629996,"d":"0.39"},{"$f":"VLOOKUP(A17099,cordwood_density!A:D,4,FALSE)","v":1.1493},{"v":0.343619291,"d":"0.34"}]
["22055","22","LA","055","Lafayette","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1358.12552974616,"A","CEC Survey",2017,15,"I",416.641181565908,"TON",8,{"v":0.3067766362096,"d":"0.31"},{"$f":"VLOOKUP(A17116,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.255179368,"d":"0.26"}]
["22059","22","LA","059","LaSalle","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",201.7220605452,"A","CEC Survey",2017,15,"I",74.29697765894738,"TON",8,{"v":0.36831359672880004,"d":"0.37"},{"$f":"VLOOKUP(A17139,cordwood_density!A:D,4,FALSE)","v":1.3612},{"v":0.27058007400000006,"d":"0.27"}]
["22061","22","LA","061","Lincoln","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",318.12576579,"A","CEC Survey",2017,15,"I",105.74313023855957,"TON",8,{"$f":"P17155/J17155","v":{"v":0.33239410827340005,"d":"0.33"}},{"$f":"VLOOKUP(A17155,cordwood_density!A:D,4,FALSE)","v":1.2289},{"$f":"S17155/T17155","v":{"v":0.270481006,"d":"0.27"}}]
["22067","22","LA","067","Morehouse","","2104008610","Hydronic heater: outdoor","Hydronic heater",32.804398281762055,"A","CEC Survey",2017,15,"I",28.313069353660822,"TON",8,{"v":0.8630875991223947,"d":"0.86"},{"$f":"VLOOKUP(A17194,cordwood_density!A:D,4,FALSE)","v":1.3002},{"v":0.6638114129536954,"d":"0.66"}]
["22067","22","LA","067","Morehouse","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",297.4020142809,"A","CEC Survey",2017,15,"I",144.01071912031256,"TON",8,{"v":0.48422913163020004,"d":"0.48"},{"$f":"VLOOKUP(A17204,cordwood_density!A:D,4,FALSE)","v":1.3002},{"v":0.372426651,"d":"0.37"}]
["22071","22","LA","071","Orleans","","2104009000","Wax Log; Total: All Combustor Types",null,986.602480014112,"A","CEC Survey",2017,15,"I",230.99550783140805,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A17233,cordwood_density!A:D,4,FALSE)","v":1.2839},{"v":0.1823602305475504,"d":"0.18"}]
["22073","22","LA","073","Ouachita","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1739.8820322307797,"A","CEC Survey",2017,15,"I",854.8044027363648,"TON",8,{"v":0.49130020708379996,"d":"0.49"},{"$f":"VLOOKUP(A17250,cordwood_density!A:D,4,FALSE)","v":1.4382},{"v":0.341607709,"d":"0.34"}]
["22077","22","LA","077","Pointe Coupee","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",293.31946622864996,"A","CEC Survey",2017,15,"I",149.09244542205124,"TON",8,{"v":0.5082937294923,"d":"0.51"},{"$f":"VLOOKUP(A17280,cordwood_density!A:D,4,FALSE)","v":1.3527},{"v":0.375762349,"d":"0.38"}]
["22079","22","LA","079","Rapides","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1480.783118246211,"A","CEC Survey",2017,15,"I",507.85785290358456,"TON",8,{"v":0.3429657231,"d":"0.34"},{"$f":"VLOOKUP(A17289,cordwood_density!A:D,4,FALSE)","v":1.4025},{"v":0.24453883999999998,"d":"0.24"}]
["22081","22","LA","081","Red River","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",165.50681205267998,"A","CEC Survey",2017,15,"I",86.50475714749936,"TON",8,{"v":0.52266584121,"d":"0.52"},{"$f":"VLOOKUP(A17310,cordwood_density!A:D,4,FALSE)","v":1.2039},{"v":0.4341439,"d":"0.43"}]
["22085","22","LA","085","Sabine","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",266.11778645826,"A","CEC Survey",2017,15,"I",75.2787249141395,"TON",8,{"v":0.282877465336,"d":"0.28"},{"$f":"VLOOKUP(A17333,cordwood_density!A:D,4,FALSE)","v":1.2535},{"v":0.225670096,"d":"0.23"}]
["22089","22","LA","089","St Charles","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",511.562148125,"A","CEC Survey",2017,15,"I",18.582379929157295,"TON",8,{"v":0.036324775,"d":"0.04"},{"$f":"VLOOKUP(A17367,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.02814564931039826,"d":"0.03"}]
["22093","22","LA","093","St James","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.3307463965850106,"A","CEC Survey",2017,15,"I",0.8768226429998716,"TON",8,{"v":0.6588953727396838,"d":"0.66"},{"$f":"VLOOKUP(A17388,cordwood_density!A:D,4,FALSE)","v":1.1},{"v":0.5989957933997125,"d":"0.60"}]
["22095","22","LA","095","St John The Baptist","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",457.56965667874994,"A","CEC Survey",2017,15,"I",97.41074823416048,"TON",8,{"v":0.21288725511479997,"d":"0.21"},{"$f":"VLOOKUP(A17409,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.164952158,"d":"0.16"}]
["22097","22","LA","097","St Landry","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",639.9810816406471,"A","CEC Survey",2017,15,"I",142.61546855806745,"TON",8,{"v":0.2228432568545,"d":"0.22"},{"$f":"VLOOKUP(A17423,cordwood_density!A:D,4,FALSE)","v":1.2967},{"v":0.171854135,"d":"0.17"}]
["22099","22","LA","099","St Martin","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",596.75503628325,"A","CEC Survey",2017,15,"I",261.7798609102723,"TON",8,{"v":0.4386722272856,"d":"0.44"},{"$f":"VLOOKUP(A17444,cordwood_density!A:D,4,FALSE)","v":1.1704},{"v":0.374805389,"d":"0.37"}]
["22105","22","LA","105","Tangipahoa","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1136.06898451134,"A","CEC Survey",2017,15,"I",304.5686764767838,"TON",8,{"v":0.2680899493156999,"d":"0.27"},{"$f":"VLOOKUP(A17483,cordwood_density!A:D,4,FALSE)","v":1.2931},{"v":0.20732344699999994,"d":"0.21"}]
["22107","22","LA","107","Tensas","","2104008620","Hydronic heater: indoor","Hydronic heater",5.91545196348101,"A","CEC Survey",2017,15,"I",4.561441199427321,"TON",8,{"v":0.7711061179411713,"d":"0.77"},{"$f":"VLOOKUP(A17495,cordwood_density!A:D,4,FALSE)","v":1.1838},{"v":0.6513820898303526,"d":"0.65"}]
["22111","22","LA","111","Union","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",42.288935621227004,"A","CEC Survey",2017,15,"I",37.71255412937463,"TON",8,{"v":0.8917830060126827,"d":"0.89"},{"$f":"VLOOKUP(A17522,cordwood_density!A:D,4,FALSE)","v":1.2889},{"v":0.6918946435042926,"d":"0.69"}]
["22113","22","LA","113","Vermilion","","2104008610","Hydronic heater: outdoor","Hydronic heater",44.22125257782858,"A","CEC Survey",2017,15,"I",36.61177705323088,"TON",8,{"$f":"P17539/J17539","v":{"v":0.8279226597843387,"d":"0.83"}},{"$f":"VLOOKUP(A17539,cordwood_density!A:D,4,FALSE)","v":1.2906},{"$f":"S17539/T17539","v":{"v":0.6415021383731122,"d":"0.64"}}]
["22117","22","LA","117","Washington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.801104312938503,"A","CEC Survey",2017,15,"I",1.4401414586549404,"TON",8,{"v":0.799588035134594,"d":"0.80"},{"$f":"VLOOKUP(A17571,cordwood_density!A:D,4,FALSE)","v":1.2358},{"v":0.6470205819182667,"d":"0.65"}]
["22117","22","LA","117","Washington","","2104009000","Wax Log; Total: All Combustor Types",null,251.95525792285653,"A","CEC Survey",2017,15,"I",58.99086403457162,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A17578,cordwood_density!A:D,4,FALSE)","v":1.2358},{"v":0.1894580838323353,"d":"0.19"}]
["22123","22","LA","123","West Carroll","","2104008100","Fireplace: general","Fireplace: general",257.810969958,"A","CEC Survey",2017,15,"I",44.2205494342045,"TON",8,{"v":0.1715231490786,"d":"0.17"},{"$f":"VLOOKUP(A17617,cordwood_density!A:D,4,FALSE)","v":1.1979},{"v":0.143186534,"d":"0.14"}]
["22123","22","LA","123","West Carroll","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",154.11625235712,"A","CEC Survey",2017,15,"I",73.23341919778998,"TON",8,{"v":0.4751829743957999,"d":"0.48"},{"$f":"VLOOKUP(A17624,cordwood_density!A:D,4,FALSE)","v":1.1979},{"v":0.3966800019999999,"d":"0.40"}]
["22127","22","LA","127","Winn","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",183.12650856864002,"A","CEC Survey",2017,15,"I",103.34377399524028,"TON",8,{"v":0.5643299531182001,"d":"0.56"},{"$f":"VLOOKUP(A17656,cordwood_density!A:D,4,FALSE)","v":1.3259},{"v":0.42562029800000006,"d":"0.43"}]
["23003","23","ME","003","Aroostook","","2104008100","Fireplace: general","Fireplace: general",2703.0144433319997,"A","CEC Survey",2017,15,"I",1618.9534098433955,"TON",8,{"v":0.5989436770629,"d":"0.60"},{"$f":"VLOOKUP(A17677,cordwood_density!A:D,4,FALSE)","v":1.1883},{"v":0.504034063,"d":"0.50"}]
["23005","23","ME","005","Cumberland","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",8289.3212746435,"A","CEC Survey",2017,15,"I",19707.808608723753,"TON",8,{"v":2.3774936398000004,"d":"2.38"},{"$f":"VLOOKUP(A17700,cordwood_density!A:D,4,FALSE)","v":1.2008},{"v":1.9799247500000001,"d":"1.98"}]
["23007","23","ME","007","Franklin","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",512.52849279,"A","CEC Survey",2017,15,"I",3060.2184202521635,"TON",8,{"v":5.970825941,"d":"5.97"},{"$f":"VLOOKUP(A17712,cordwood_density!A:D,4,FALSE)","v":1.2102},{"v":4.933751397289704,"d":"4.93"}]
["23011","23","ME","011","Kennebec","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",89.65034071519673,"A","CEC Survey",2017,15,"I",469.8492039953492,"TON",8,{"v":5.240908180014363,"d":"5.24"},{"$f":"VLOOKUP(A17733,cordwood_density!A:D,4,FALSE)","v":1.1913},{"v":4.399318542780461,"d":"4.40"}]
["23015","23","ME","015","Lincoln","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1323.2322418337003,"A","CEC Survey",2017,15,"I",3769.7421466779106,"TON",8,{"v":2.848889278463999,"d":"2.85"},{"$f":"VLOOKUP(A17776,cordwood_density!A:D,4,FALSE)","v":1.1904},{"v":2.3932201599999994,"d":"2.39"}]
["23019","23","ME","019","Penobscot","","2104008610","Hydronic heater: outdoor","Hydronic heater",1228.0630445391846,"A","CEC Survey",2017,15,"I",6506.808712802071,"TON",8,{"v":5.298432146245122,"d":"5.30"},{"$f":"VLOOKUP(A17794,cordwood_density!A:D,4,FALSE)","v":1.1888},{"v":4.456958400273487,"d":"4.46"}]
["23021","23","ME","021","Piscataquis","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",11.150618474374728,"A","CEC Survey",2017,15,"I",65.69152383449217,"TON",8,{"v":5.891289706078464,"d":"5.89"},{"$f":"VLOOKUP(A17811,cordwood_density!A:D,4,FALSE)","v":1.1972},{"v":4.920890165451439,"d":"4.92"}]
["23023","23","ME","023","Sagadahoc","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",632.402837895,"A","CEC Survey",2017,15,"I",679.2065887468876,"TON",8,{"v":1.0740093940876,"d":"1.07"},{"$f":"VLOOKUP(A17829,cordwood_density!A:D,4,FALSE)","v":1.1954},{"v":0.898451894,"d":"0.90"}]
["23025","23","ME","025","Somerset","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3209.03969736,"A","CEC Survey",2017,15,"I",10368.907256481483,"TON",8,{"v":3.2311558080792,"d":"3.23"},{"$f":"VLOOKUP(A17850,cordwood_density!A:D,4,FALSE)","v":1.1898},{"v":2.715713404,"d":"2.72"}]
["23029","23","ME","029","Washington","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",419.75116947843634,"A","CEC Survey",2017,15,"I",2272.72997730074,"TON",8,{"v":5.414469672889132,"d":"5.41"},{"$f":"VLOOKUP(A17867,cordwood_density!A:D,4,FALSE)","v":1.1979},{"v":4.519968004749255,"d":"4.52"}]
["24001","24","MD","001","Allegany","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3980.2063382039996,"A","CEC Survey",2017,15,"I",1586.5075955461148,"TON",8,{"v":0.39859933398880004,"d":"0.40"},{"$f":"VLOOKUP(A17906,cordwood_density!A:D,4,FALSE)","v":1.2236},{"v":0.32575950800000003,"d":"0.33"}]
["24003","24","MD","003","Anne Arundel","","2104008620","Hydronic heater: indoor","Hydronic heater",380.0773104208103,"A","CEC Survey",2017,15,"I",684.7960795501538,"TON",8,{"v":1.8017283872903855,"d":"1.80"},{"$f":"VLOOKUP(A17915,cordwood_density!A:D,4,FALSE)","v":1.2104},{"v":1.4885396458116207,"d":"1.49"}]
["24009","24","MD","009","Calvert","","2104008620","Hydronic heater: indoor","Hydronic heater",113.51662083399364,"A","CEC Survey",2017,15,"I",378.26116682083057,"TON",8,{"v":3.332209539376604,"d":"3.33"},{"$f":"VLOOKUP(A17945,cordwood_density!A:D,4,FALSE)","v":1.1559},{"v":2.8827835793551384,"d":"2.88"}]
["24011","24","MD","011","Caroline","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1895.4475454760002,"A","CEC Survey",2017,15,"I",752.7589816177982,"TON",8,{"v":0.39714049772279997,"d":"0.40"},{"$f":"VLOOKUP(A17966,cordwood_density!A:D,4,FALSE)","v":1.2051},{"v":0.32954982799999993,"d":"0.33"}]
["24015","24","MD","015","Cecil","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.961053438627903,"A","CEC Survey",2017,15,"I",20.291472478120596,"TON",8,{"v":3.4040078128860434,"d":"3.40"},{"$f":"VLOOKUP(A17991,cordwood_density!A:D,4,FALSE)","v":1.1445},{"v":2.9742313786684518,"d":"2.97"}]
["24015","24","MD","015","Cecil","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1204.0936891357162,"A","CEC Survey",2017,15,"I",1985.8956024813735,"TON",8,{"v":1.6492866131595003,"d":"1.65"},{"$f":"VLOOKUP(A18001,cordwood_density!A:D,4,FALSE)","v":1.1445},{"v":1.4410542710000003,"d":"1.44"}]
["24021","24","MD","021","Frederick","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",2482.4315548812983,"A","CEC Survey",2017,15,"I",4325.543881475312,"TON",8,{"v":1.742462495278,"d":"1.74"},{"$f":"VLOOKUP(A18044,cordwood_density!A:D,4,FALSE)","v":1.322},{"v":1.3180502989999998,"d":"1.32"}]
["24025","24","MD","025","Harford","","2104008100","Fireplace: general","Fireplace: general",8088.657109949269,"A","CEC Survey",2017,15,"I",3712.7838197230185,"TON",8,{"v":0.45901115219190003,"d":"0.46"},{"$f":"VLOOKUP(A18067,cordwood_density!A:D,4,FALSE)","v":1.2047},{"v":0.381016977,"d":"0.38"}]
["24027","24","MD","027","Howard","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1316.7293084550201,"A","CEC Survey",2017,15,"I",1199.9972239778326,"TON",8,{"v":0.911346938412,"d":"0.91"},{"$f":"VLOOKUP(A18083,cordwood_density!A:D,4,FALSE)","v":1.1838},{"v":0.76984874,"d":"0.77"}]
["24029","24","MD","029","Kent","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",154.3473508122,"A","CEC Survey",2017,15,"I",103.8775641285819,"TON",8,{"v":0.6730116427782001,"d":"0.67"},{"$f":"VLOOKUP(A18100,cordwood_density!A:D,4,FALSE)","v":1.2738},{"v":0.528349539,"d":"0.53"}]
["24031","24","MD","031","Montgomery","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6987.079994803636,"A","CEC Survey",2017,15,"I",7469.499001911024,"TON",8,{"v":1.0690444373710002,"d":"1.07"},{"$f":"VLOOKUP(A18120,cordwood_density!A:D,4,FALSE)","v":1.1566},{"v":0.9242991850000001,"d":"0.92"}]
["24035","24","MD","035","Queen Annes","","2104008610","Hydronic heater: outdoor","Hydronic heater",120.54074593096017,"A","CEC Survey",2017,15,"I",461.9159102238211,"TON",8,{"v":3.832031290800074,"d":"3.83"},{"$f":"VLOOKUP(A18139,cordwood_density!A:D,4,FALSE)","v":1.2818},{"v":2.98957036261513,"d":"2.99"}]
["24039","24","MD","039","Somerset","","2104009000","Wax Log; Total: All Combustor Types",null,28.643578302684464,"A","CEC Survey",2017,15,"I",4.010100962375826,"TON",8,0.14,{"$f":"VLOOKUP(A18178,cordwood_density!A:D,4,FALSE)","v":1.1805},{"v":0.11859381617958492,"d":"0.12"}]
["24041","24","MD","041","Talbot","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",538.3771526123201,"A","CEC Survey",2017,15,"I",918.8021173817717,"TON",8,{"v":1.7066142441661,"d":"1.71"},{"$f":"VLOOKUP(A18196,cordwood_density!A:D,4,FALSE)","v":1.1933},{"v":1.430163617,"d":"1.43"}]
["24045","24","MD","045","Wicomico","","2104008100","Fireplace: general","Fireplace: general",2923.4646508900005,"A","CEC Survey",2017,15,"I",1398.0481136991543,"TON",8,{"v":0.478216185468,"d":"0.48"},{"$f":"VLOOKUP(A18217,cordwood_density!A:D,4,FALSE)","v":1.2093},{"v":0.39544875999999995,"d":"0.40"}]
["24047","24","MD","047","Worcester","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",356.0385953267,"A","CEC Survey",2017,15,"I",277.9971266869513,"TON",8,{"v":0.7808061551075999,"d":"0.78"},{"$f":"VLOOKUP(A18234,cordwood_density!A:D,4,FALSE)","v":1.1931},{"v":0.6544347959999999,"d":"0.65"}]
["24510","24","MD","510","Baltimore City","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1748.2271250205097,"A","CEC Survey",2017,15,"I",807.737947955721,"TON",8,{"v":0.46203261372360005,"d":"0.46"},{"$f":"VLOOKUP(A18255,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.35799830600000004,"d":"0.36"}]
["25003","25","MA","003","Berkshire","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1534.53587999,"A","CEC Survey",2017,15,"I",1922.2615686831589,"TON",8,{"v":1.252666421,"d":"1.25"},{"$f":"VLOOKUP(A18282,cordwood_density!A:D,4,FALSE)","v":1.275},{"v":0.9824834674509805,"d":"0.98"}]
["25007","25","MA","007","Dukes","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",248.62869575050013,"A","CEC Survey",2017,15,"I",116.45377811626837,"TON",8,{"v":0.468384302,"d":"0.47"},{"$f":"VLOOKUP(A18312,cordwood_density!A:D,4,FALSE)","v":1.1798},{"v":0.3970031378199695,"d":"0.40"}]
["25011","25","MA","011","Franklin","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",33.22063765031396,"A","CEC Survey",2017,15,"I",100.4860203104973,"TON",8,{"v":3.0248070903463717,"d":"3.02"},{"$f":"VLOOKUP(A18333,cordwood_density!A:D,4,FALSE)","v":1.2723},{"v":2.3774322803948533,"d":"2.38"}]
["25011","25","MA","011","Franklin","","2104008620","Hydronic heater: indoor","Hydronic heater",254.6915553190737,"A","CEC Survey",2017,15,"I",770.3928223804794,"TON",8,{"v":3.024807090346372,"d":"3.02"},{"$f":"VLOOKUP(A18335,cordwood_density!A:D,4,FALSE)","v":1.2723},{"v":2.3774322803948538,"d":"2.38"}]
["25015","25","MA","015","Hampshire","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",583.65836607168,"A","CEC Survey",2017,15,"I",570.442094156346,"TON",8,{"v":0.9773561509890002,"d":"0.98"},{"$f":"VLOOKUP(A18368,cordwood_density!A:D,4,FALSE)","v":1.193},{"v":0.8192423730000001,"d":"0.82"}]
["25017","25","MA","017","Middlesex","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",5258.939295342175,"A","CEC Survey",2017,15,"I",4774.237644252347,"TON",8,{"v":0.907832811168,"d":"0.91"},{"$f":"VLOOKUP(A18389,cordwood_density!A:D,4,FALSE)","v":1.0944},{"v":0.8295255949999999,"d":"0.83"}]
["25021","25","MA","021","Norfolk","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",34.06217288023911,"A","CEC Survey",2017,15,"I",10.742096449689427,"TON",8,{"v":0.3153673280755781,"d":"0.32"},{"$f":"VLOOKUP(A18411,cordwood_density!A:D,4,FALSE)","v":0.8643},{"v":0.3648817865041977,"d":"0.36"}]
["25023","25","MA","023","Plymouth","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1438.9694462616,"A","CEC Survey",2017,15,"I",650.269876148132,"TON",8,{"v":0.45189971047509997,"d":"0.45"},{"$f":"VLOOKUP(A18428,cordwood_density!A:D,4,FALSE)","v":0.8891},{"v":0.508266461,"d":"0.51"}]
["26001","26","MI","001","Alcona","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",148.51947920230035,"A","CEC Survey",2017,15,"I",395.8748380313048,"TON",8,{"v":2.6654741866693357,"d":"2.67"},{"$f":"VLOOKUP(A18467,cordwood_density!A:D,4,FALSE)","v":1.1725},{"v":2.2733255323405848,"d":"2.27"}]
["26003","26","MI","003","Alger","","2104008100","Fireplace: general","Fireplace: general",493.68764042400005,"A","CEC Survey",2017,15,"I",181.44588804965719,"TON",8,{"v":0.36753176136599996,"d":"0.37"},{"$f":"VLOOKUP(A18487,cordwood_density!A:D,4,FALSE)","v":1.386},{"v":0.265174431,"d":"0.27"}]
["26005","26","MI","005","Allegan","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,6366.787458332096,"A","CEC Survey",2017,15,"I",1762.381410199172,"TON",8,{"v":0.27680858230829997,"d":"0.28"},{"$f":"VLOOKUP(A18506,cordwood_density!A:D,4,FALSE)","v":1.3153},{"v":0.210452811,"d":"0.21"}]
["26007","26","MI","007","Alpena","","2104009000","Wax Log; Total: All Combustor Types",null,12.455348583091942,"A","CEC Survey",2017,15,"I",6.862897069283661,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A18523,cordwood_density!A:D,4,FALSE)","v":1.1518},{"v":0.4783816634832437,"d":"0.48"}]
["26011","26","MI","011","Arenac","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",331.78479794099997,"A","CEC Survey",2017,15,"I",236.9817103075134,"TON",8,{"v":0.714263317,"d":"0.71"},{"$f":"VLOOKUP(A18552,cordwood_density!A:D,4,FALSE)","v":1.2737},{"v":0.5607782970872262,"d":"0.56"}]
["26013","26","MI","013","Baraga","","2104008100","Fireplace: general","Fireplace: general",490.693797357,"A","CEC Survey",2017,15,"I",188.46356417170702,"TON",8,{"v":0.38407570095,"d":"0.38"},{"$f":"VLOOKUP(A18562,cordwood_density!A:D,4,FALSE)","v":1.3875},{"v":0.276811316,"d":"0.28"}]
["26017","26","MI","017","Bay","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1390.1298696284998,"A","CEC Survey",2017,15,"I",1694.3780725045522,"TON",8,{"v":1.2188631505036,"d":"1.22"},{"$f":"VLOOKUP(A18601,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.937154506,"d":"0.94"}]
["26019","26","MI","019","Benzie","","2104008620","Hydronic heater: indoor","Hydronic heater",106.87398257174743,"A","CEC Survey",2017,15,"I",303.49914363535987,"TON",8,{"v":2.839785103279113,"d":"2.84"},{"$f":"VLOOKUP(A18605,cordwood_density!A:D,4,FALSE)","v":1.3053},{"v":2.1755804054846495,"d":"2.18"}]
["26023","26","MI","023","Branch","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",292.94446032599996,"A","CEC Survey",2017,15,"I",132.40123254058204,"TON",8,{"v":0.45196701242700005,"d":"0.45"},{"$f":"VLOOKUP(A18640,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.34750654500000006,"d":"0.35"}]
["26025","26","MI","025","Calhoun","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1631.6546809200001,"A","CEC Survey",2017,15,"I",688.3375761044441,"TON",8,{"v":0.421864739,"d":"0.42"},{"$f":"VLOOKUP(A18657,cordwood_density!A:D,4,FALSE)","v":1.4437},{"v":0.29221080487635936,"d":"0.29"}]
["26029","26","MI","029","Charlevoix","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.138202482837604,"A","CEC Survey",2017,15,"I",38.18861310486436,"TON",8,{"v":2.7010939439593966,"d":"2.70"},{"$f":"VLOOKUP(A18678,cordwood_density!A:D,4,FALSE)","v":1.2746},{"v":2.1191698916988835,"d":"2.12"}]
["26031","26","MI","031","Cheboygan","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",540.050366768,"A","CEC Survey",2017,15,"I",551.7713175001273,"TON",8,{"v":1.02170344,"d":"1.02"},{"$f":"VLOOKUP(A18702,cordwood_density!A:D,4,FALSE)","v":1.2005},{"v":0.8510649229487715,"d":"0.85"}]
["26033","26","MI","033","Chippewa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",530.949980664,"A","CEC Survey",2017,15,"I",636.2917937597889,"TON",8,{"v":1.198402518,"d":"1.20"},{"$f":"VLOOKUP(A18717,cordwood_density!A:D,4,FALSE)","v":1.2161},{"v":0.985447346435326,"d":"0.99"}]
["26039","26","MI","039","Crawford","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.165831333328867,"A","CEC Survey",2017,15,"I",12.2895778809667,"TON",8,{"v":2.9500901255035314,"d":"2.95"},{"$f":"VLOOKUP(A18756,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2682532104440503,"d":"2.27"}]
["26041","26","MI","041","Delta","","2104009000","Wax Log; Total: All Combustor Types",null,15.504664120949544,"A","CEC Survey",2017,15,"I",8.543069930643199,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A18778,cordwood_density!A:D,4,FALSE)","v":1.2887},{"v":0.42756266004500665,"d":"0.43"}]
["26043","26","MI","043","Dickinson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",943.6144629677701,"A","CEC Survey",2017,15,"I",1384.2471363759598,"TON",8,{"v":1.4669626110036,"d":"1.47"},{"$f":"VLOOKUP(A18795,cordwood_density!A:D,4,FALSE)","v":1.2163},{"v":1.206086172,"d":"1.21"}]
["26047","26","MI","047","Emmet","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",238.3100133207484,"A","CEC Survey",2017,15,"I",641.7923920655508,"TON",8,{"v":2.6930987209578294,"d":"2.69"},{"$f":"VLOOKUP(A18812,cordwood_density!A:D,4,FALSE)","v":1.2618},{"v":2.1343308931350684,"d":"2.13"}]
["26051","26","MI","051","Gladwin","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",17.55810006840629,"A","CEC Survey",2017,15,"I",49.23044327218279,"TON",8,{"v":2.803859362936831,"d":"2.80"},{"$f":"VLOOKUP(A18843,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.1558199007664394,"d":"2.16"}]
["26051","26","MI","051","Gladwin","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1848.94656604,"A","CEC Survey",2017,15,"I",508.9823880571896,"TON",8,{"v":0.2752823674874,"d":"0.28"},{"$f":"VLOOKUP(A18851,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.211657979,"d":"0.21"}]
["26057","26","MI","057","Gratiot","","2104008620","Hydronic heater: indoor","Hydronic heater",111.26232822349392,"A","CEC Survey",2017,15,"I",320.6560645574775,"TON",8,{"v":2.881982335596753,"d":"2.88"},{"$f":"VLOOKUP(A18890,cordwood_density!A:D,4,FALSE)","v":1.4148},{"v":2.0370245515951035,"d":"2.04"}]
["26057","26","MI","057","Gratiot","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2187.614784192,"A","CEC Survey",2017,15,"I",650.2287216895616,"TON",8,{"v":0.2972318190516,"d":"0.30"},{"$f":"VLOOKUP(A18896,cordwood_density!A:D,4,FALSE)","v":1.4148},{"v":0.210087517,"d":"0.21"}]
["26061","26","MI","061","Houghton","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",244.27211099844,"A","CEC Survey",2017,15,"I",419.4095669492137,"TON",8,{"v":1.7169768797384002,"d":"1.72"},{"$f":"VLOOKUP(A18929,cordwood_density!A:D,4,FALSE)","v":1.4249},{"v":1.204980616,"d":"1.20"}]
["26063","26","MI","063","Huron","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",743.660711374,"A","CEC Survey",2017,15,"I",1179.7217369277919,"TON",8,{"v":1.5863709335244,"d":"1.59"},{"$f":"VLOOKUP(A18946,cordwood_density!A:D,4,FALSE)","v":1.4268},{"v":1.111838333,"d":"1.11"}]
["26067","26","MI","067","Ionia","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",854.03144075,"A","CEC Survey",2017,15,"I",447.54895234389727,"TON",8,{"v":0.524042712,"d":"0.52"},{"$f":"VLOOKUP(A18972,cordwood_density!A:D,4,FALSE)","v":1.322},{"v":0.39640144629349466,"d":"0.40"}]
["26069","26","MI","069","Iosco","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",227.72584244025,"A","CEC Survey",2017,15,"I",134.90249183103123,"TON",8,{"v":0.5923899122974,"d":"0.59"},{"$f":"VLOOKUP(A18985,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.455474329,"d":"0.46"}]
["26071","26","MI","071","Iron","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",407.23467734775,"A","CEC Survey",2017,15,"I",758.4245177610389,"TON",8,{"v":1.8623770517298,"d":"1.86"},{"$f":"VLOOKUP(A19006,cordwood_density!A:D,4,FALSE)","v":1.3938},{"v":1.336186721,"d":"1.34"}]
["26077","26","MI","077","Kalamazoo","","2104009000","Wax Log; Total: All Combustor Types",null,99.69148421787922,"A","CEC Survey",2017,15,"I",54.930007804051456,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A19048,cordwood_density!A:D,4,FALSE)","v":1.2869},{"v":0.4281606962467947,"d":"0.43"}]
["26079","26","MI","079","Kalkaska","","2104009000","Wax Log; Total: All Combustor Types",null,6.835881750310606,"A","CEC Survey",2017,15,"I",3.7665708444211443,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A19063,cordwood_density!A:D,4,FALSE)","v":1.2478},{"v":0.4415771758294599,"d":"0.44"}]
["26083","26","MI","083","Keweenaw","","2104008610","Hydronic heater: outdoor","Hydronic heater",35.994296241143076,"A","CEC Survey",2017,15,"I",118.06821367956914,"TON",8,{"v":3.280192308486141,"d":"3.28"},{"$f":"VLOOKUP(A19084,cordwood_density!A:D,4,FALSE)","v":1.4005},{"v":2.34215802105401,"d":"2.34"}]
["26085","26","MI","085","Lake","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.0453503384082983,"A","CEC Survey",2017,15,"I",9.135728237407154,"TON",8,{"v":2.999894009627178,"d":"3.00"},{"$f":"VLOOKUP(A19101,cordwood_density!A:D,4,FALSE)","v":1.3122},{"v":2.2861560811059123,"d":"2.29"}]
["26087","26","MI","087","Lapeer","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1473.671775744,"A","CEC Survey",2017,15,"I",792.3181698200318,"TON",8,{"v":0.537649009,"d":"0.54"},{"$f":"VLOOKUP(A19122,cordwood_density!A:D,4,FALSE)","v":1.2545},{"v":0.42857633240334797,"d":"0.43"}]
["26089","26","MI","089","Leelanau","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",866.2166252469601,"A","CEC Survey",2017,15,"I",1310.9687585380336,"TON",8,{"v":1.5134421579178001,"d":"1.51"},{"$f":"VLOOKUP(A19140,cordwood_density!A:D,4,FALSE)","v":1.3229},{"v":1.144033682,"d":"1.14"}]
["26095","26","MI","095","Luce","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",89.12610860604,"A","CEC Survey",2017,15,"I",59.455976289848884,"TON",8,{"v":0.667099430456,"d":"0.67"},{"$f":"VLOOKUP(A19179,cordwood_density!A:D,4,FALSE)","v":1.1356},{"v":0.58744226,"d":"0.59"}]
["26097","26","MI","097","Mackinac","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",152.86343578990457,"A","CEC Survey",2017,15,"I",483.72245450559706,"TON",8,{"v":3.16440914732824,"d":"3.16"},{"$f":"VLOOKUP(A19187,cordwood_density!A:D,4,FALSE)","v":1.3573},{"v":2.331399946458587,"d":"2.33"}]
["26101","26","MI","101","Manistee","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",14.086802343673195,"A","CEC Survey",2017,15,"I",37.996817768931685,"TON",8,{"v":2.6973344867011066,"d":"2.70"},{"$f":"VLOOKUP(A19218,cordwood_density!A:D,4,FALSE)","v":1.2601},{"v":2.1405717694636195,"d":"2.14"}]
["26103","26","MI","103","Marquette","","2104008620","Hydronic heater: indoor","Hydronic heater",354.3656946571676,"A","CEC Survey",2017,15,"I",1118.9107959420821,"TON",8,{"v":3.1575031466422745,"d":"3.16"},{"$f":"VLOOKUP(A19235,cordwood_density!A:D,4,FALSE)","v":1.3888},{"v":2.2735477726398865,"d":"2.27"}]
["26107","26","MI","107","Mecosta","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",19.118019992335288,"A","CEC Survey",2017,15,"I",52.53135743915172,"TON",8,{"v":2.7477404804583507,"d":"2.75"},{"$f":"VLOOKUP(A19263,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.1126714443013617,"d":"2.11"}]
["26107","26","MI","107","Mecosta","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",293.19589547328,"A","CEC Survey",2017,15,"I",447.6031205260276,"TON",8,{"v":1.5266350158261996,"d":"1.53"},{"$f":"VLOOKUP(A19274,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.1737928769999997,"d":"1.17"}]
["26111","26","MI","111","Midland","","2104008620","Hydronic heater: indoor","Hydronic heater",227.00110666695062,"A","CEC Survey",2017,15,"I",601.522553815864,"TON",8,{"v":2.64986617311254,"d":"2.65"},{"$f":"VLOOKUP(A19295,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.0374182478183456,"d":"2.04"}]
["26117","26","MI","117","Montcalm","","2104008610","Hydronic heater: outdoor","Hydronic heater",369.6363951492568,"A","CEC Survey",2017,15,"I",1047.9174855283104,"TON",8,{"v":2.8349954151705434,"d":"2.83"},{"$f":"VLOOKUP(A19339,cordwood_density!A:D,4,FALSE)","v":1.3506},{"v":2.0990636866359718,"d":"2.10"}]
["26119","26","MI","119","Montmorency","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",124.26838549739583,"A","CEC Survey",2017,15,"I",322.2230811078981,"TON",8,{"v":2.592961032028944,"d":"2.59"},{"$f":"VLOOKUP(A19352,cordwood_density!A:D,4,FALSE)","v":1.1527},{"v":2.2494673653413235,"d":"2.25"}]
["26121","26","MI","121","Muskegon","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",341.17734487295996,"A","CEC Survey",2017,15,"I",203.00220034771667,"TON",8,{"v":0.5950049245600001,"d":"0.60"},{"$f":"VLOOKUP(A19373,cordwood_density!A:D,4,FALSE)","v":1.36},{"v":0.437503621,"d":"0.44"}]
["26123","26","MI","123","Newaygo","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",777.2769048199999,"A","CEC Survey",2017,15,"I",819.9758988233649,"TON",8,{"v":1.054934083,"d":"1.05"},{"$f":"VLOOKUP(A19392,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.8111133961248654,"d":"0.81"}]
["26125","26","MI","125","Oakland","","2104009000","Wax Log; Total: All Combustor Types",null,12756.203683332376,"A","CEC Survey",2017,15,"I",7116.677048058075,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A19408,cordwood_density!A:D,4,FALSE)","v":1.2613},{"v":0.4423208558550701,"d":"0.44"}]
["26129","26","MI","129","Ogemaw","","2104008610","Hydronic heater: outdoor","Hydronic heater",265.70214457715434,"A","CEC Survey",2017,15,"I",782.2979083354819,"TON",8,{"v":2.944266443842417,"d":"2.94"},{"$f":"VLOOKUP(A19429,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2637755219455764,"d":"2.26"}]
["26133","26","MI","133","Osceola","","2104009000","Wax Log; Total: All Combustor Types",null,8.774938677466084,"A","CEC Survey",2017,15,"I",4.834991211283812,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A19468,cordwood_density!A:D,4,FALSE)","v":1.1781},{"v":0.4677022324081148,"d":"0.47"}]
["26137","26","MI","137","Otsego","","2104008620","Hydronic heater: indoor","Hydronic heater",131.81998237654372,"A","CEC Survey",2017,15,"I",343.5559022792471,"TON",8,{"v":2.6062505553815036,"d":"2.61"},{"$f":"VLOOKUP(A19490,cordwood_density!A:D,4,FALSE)","v":1.1795},{"v":2.2096231923539666,"d":"2.21"}]
["26139","26","MI","139","Ottawa","","2104008100","Fireplace: general","Fireplace: general",12508.229501971,"A","CEC Survey",2017,15,"I",3646.580653907217,"TON",8,{"v":0.2915345176016,"d":"0.29"},{"$f":"VLOOKUP(A19507,cordwood_density!A:D,4,FALSE)","v":1.2656},{"v":0.230352811,"d":"0.23"}]
["26141","26","MI","141","Presque Isle","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",211.9131683669,"A","CEC Survey",2017,15,"I",115.25732098353174,"TON",8,{"v":0.5438893763504999,"d":"0.54"},{"$f":"VLOOKUP(A19524,cordwood_density!A:D,4,FALSE)","v":1.1611},{"v":0.46842595499999995,"d":"0.47"}]
["26145","26","MI","145","Saginaw","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1628.627684351936,"A","CEC Survey",2017,15,"I",715.5930286296293,"TON",8,{"v":0.4393840504525,"d":"0.44"},{"$f":"VLOOKUP(A19554,cordwood_density!A:D,4,FALSE)","v":1.1845},{"v":0.37094474499999996,"d":"0.37"}]
["26147","26","MI","147","St Clair","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",36.103659724005645,"A","CEC Survey",2017,15,"I",88.92505663127021,"TON",8,{"v":2.4630482702046725,"d":"2.46"},{"$f":"VLOOKUP(A19563,cordwood_density!A:D,4,FALSE)","v":1.3013},{"v":1.8927597557862696,"d":"1.89"}]
["26151","26","MI","151","Sanilac","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",799.4244155040001,"A","CEC Survey",2017,15,"I",447.1807592592313,"TON",8,{"v":0.559378411,"d":"0.56"},{"$f":"VLOOKUP(A19602,cordwood_density!A:D,4,FALSE)","v":1.348},{"v":0.4149691476261127,"d":"0.41"}]
["26153","26","MI","153","Schoolcraft","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",87.28683832637172,"A","CEC Survey",2017,15,"I",269.86305165710075,"TON",8,{"v":3.0916809089597623,"d":"3.09"},{"$f":"VLOOKUP(A19607,cordwood_density!A:D,4,FALSE)","v":1.3367},{"v":2.3129205573126073,"d":"2.31"}]
["26157","26","MI","157","Tuscola","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",8.751507043828044,"A","CEC Survey",2017,15,"I",23.558205350095978,"TON",8,{"v":2.691902689687062,"d":"2.69"},{"$f":"VLOOKUP(A19641,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.069739112476597,"d":"2.07"}]
["26159","26","MI","159","Van Buren","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1151.0463876018566,"A","CEC Survey",2017,15,"I",652.6588823341554,"TON",8,{"v":0.567013536,"d":"0.57"},{"$f":"VLOOKUP(A19662,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.4359630447485776,"d":"0.44"}]
["26163","26","MI","163","Wayne","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",242.0791608242182,"A","CEC Survey",2017,15,"I",1.4024341390300172,"TON",8,{"v":5.79328734557359E-3,"d":"0.01"},{"$f":"VLOOKUP(A19683,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":4.454319041652768E-3,"d":"0.00"}]
["26165","26","MI","165","Wexford","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",244.64075746758064,"A","CEC Survey",2017,15,"I",678.7469713703077,"TON",8,{"v":2.7744639870985277,"d":"2.77"},{"$f":"VLOOKUP(A19697,cordwood_density!A:D,4,FALSE)","v":1.261},{"v":2.200209347421513,"d":"2.20"}]
["27003","27","MN","003","Anoka","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6110.142407578081,"A","CEC Survey",2017,15,"I",7349.688081935982,"TON",8,{"v":1.2028669041854998,"d":"1.20"},{"$f":"VLOOKUP(A19740,cordwood_density!A:D,4,FALSE)","v":1.3513},{"v":0.8901553349999999,"d":"0.89"}]
["27007","27","MN","007","Beltrami","","2104008610","Hydronic heater: outdoor","Hydronic heater",469.360128492102,"A","CEC Survey",2017,15,"I",1382.7999716617785,"TON",8,{"v":2.946138556984495,"d":"2.95"},{"$f":"VLOOKUP(A19759,cordwood_density!A:D,4,FALSE)","v":1.1981},{"v":2.4590088949040108,"d":"2.46"}]
["27009","27","MN","009","Benton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",331.54552040775,"A","CEC Survey",2017,15,"I",140.89860752962937,"TON",8,{"$f":"P19779/J19779","v":{"v":0.42497515079180004,"d":"0.42"}},{"$f":"VLOOKUP(A19779,cordwood_density!A:D,4,FALSE)","v":1.3006},{"$f":"S19779/T19779","v":{"v":0.326753153,"d":"0.33"}}]
["27011","27","MN","011","Big Stone","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,355.01557147200003,"A","CEC Survey",2017,15,"I",103.0862092105906,"TON",8,{"v":0.29037095128859997,"d":"0.29"},{"$f":"VLOOKUP(A19796,cordwood_density!A:D,4,FALSE)","v":1.3377},{"v":0.21706731799999998,"d":"0.22"}]
["27013","27","MN","013","Blue Earth","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",653.29890015,"A","CEC Survey",2017,15,"I",332.9960927515201,"TON",8,{"v":0.509714761,"d":"0.51"},{"$f":"VLOOKUP(A19812,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.3919073973550669,"d":"0.39"}]
["27017","27","MN","017","Carlton","","2104008620","Hydronic heater: indoor","Hydronic heater",205.63358191469075,"A","CEC Survey",2017,15,"I",578.2877484359776,"TON",8,{"v":2.812224263427393,"d":"2.81"},{"$f":"VLOOKUP(A19835,cordwood_density!A:D,4,FALSE)","v":1.1705},{"v":2.402583736375389,"d":"2.40"}]
["27021","27","MN","021","Cass","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",470.15960483759994,"A","CEC Survey",2017,15,"I",791.2334984962894,"TON",8,{"v":1.6829040401495001,"d":"1.68"},{"$f":"VLOOKUP(A19874,cordwood_density!A:D,4,FALSE)","v":1.2355},{"v":1.3621238690000002,"d":"1.36"}]
["27023","27","MN","023","Chippewa","","2104009000","Wax Log; Total: All Combustor Types",null,0.6389700237706378,"A","CEC Survey",2017,15,"I",0.6249126832476838,"TON",8,{"v":0.978,"d":"0.98"},{"$f":"VLOOKUP(A19888,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.7519606335537444,"d":"0.75"}]
["27027","27","MN","027","Clay","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",102.60269192292,"A","CEC Survey",2017,15,"I",41.628522735591005,"TON",8,{"v":0.4057254439958001,"d":"0.41"},{"$f":"VLOOKUP(A19913,cordwood_density!A:D,4,FALSE)","v":1.3589},{"v":0.2985690220000001,"d":"0.30"}]
["27029","27","MN","029","Clearwater","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",87.67175080579999,"A","CEC Survey",2017,15,"I",42.778080502304846,"TON",8,{"v":0.48793459819300006,"d":"0.49"},{"$f":"VLOOKUP(A19930,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.375161155,"d":"0.38"}]
["27031","27","MN","031","Cook","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",312.512627385,"A","CEC Survey",2017,15,"I",524.0528124557551,"TON",8,{"v":1.6769012402502002,"d":"1.68"},{"$f":"VLOOKUP(A19951,cordwood_density!A:D,4,FALSE)","v":1.1943},{"v":1.4040871140000002,"d":"1.40"}]
["27035","27","MN","035","Crow Wing","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",739.6822745006001,"A","CEC Survey",2017,15,"I",365.62223315840504,"TON",8,{"v":0.4942963293330999,"d":"0.49"},{"$f":"VLOOKUP(A19974,cordwood_density!A:D,4,FALSE)","v":1.2361},{"v":0.39988377099999994,"d":"0.40"}]
["27039","27","MN","039","Dodge","","2104009000","Wax Log; Total: All Combustor Types",null,0.9790156373331781,"A","CEC Survey",2017,15,"I",0.9574772933118482,"TON",8,{"v":0.978,"d":"0.98"},{"$f":"VLOOKUP(A20008,cordwood_density!A:D,4,FALSE)","v":1.3212},{"v":0.740236148955495,"d":"0.74"}]
["27043","27","MN","043","Faribault","","2104008610","Hydronic heater: outdoor","Hydronic heater",113.84135741971063,"A","CEC Survey",2017,15,"I",329.45796990768133,"TON",8,{"v":2.894009500370193,"d":"2.89"},{"$f":"VLOOKUP(A20029,cordwood_density!A:D,4,FALSE)","v":1.2968},{"v":2.231654457410698,"d":"2.23"}]
["27045","27","MN","045","Fillmore","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",159.77673593,"A","CEC Survey",2017,15,"I",73.28958978396366,"TON",8,{"v":0.4587000063393,"d":"0.46"},{"$f":"VLOOKUP(A20050,cordwood_density!A:D,4,FALSE)","v":1.2639},{"v":0.362924287,"d":"0.36"}]
["27047","27","MN","047","Freeborn","","2104009000","Wax Log; Total: All Combustor Types",null,1.6496859074854775,"A","CEC Survey",2017,15,"I",1.613392817520797,"TON",8,{"v":0.978,"d":"0.98"},{"$f":"VLOOKUP(A20068,cordwood_density!A:D,4,FALSE)","v":1.2968},{"v":0.7541640962368908,"d":"0.75"}]
["27049","27","MN","049","Goodhue","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1269.3718521862002,"A","CEC Survey",2017,15,"I",1752.9946758504307,"TON",8,{"v":1.3809938142486,"d":"1.38"},{"$f":"VLOOKUP(A20085,cordwood_density!A:D,4,FALSE)","v":1.2758},{"v":1.082453217,"d":"1.08"}]
["27053","27","MN","053","Hennepin","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",306.5209070950062,"A","CEC Survey",2017,15,"I",15.68527321936032,"TON",8,{"v":0.051171952243044445,"d":"0.05"},{"$f":"VLOOKUP(A20103,cordwood_density!A:D,4,FALSE)","v":1.3645},{"v":0.03750234682524327,"d":"0.04"}]
["27055","27","MN","055","Houston","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",243.76508468756003,"A","CEC Survey",2017,15,"I",139.2072508739823,"TON",8,{"v":0.5710713289903999,"d":"0.57"},{"$f":"VLOOKUP(A20124,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.43908298399999995,"d":"0.44"}]
["27061","27","MN","061","Itasca","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",57.79963789439547,"A","CEC Survey",2017,15,"I",166.53733669149605,"TON",8,{"$f":"P20163/J20163","v":{"v":2.881286851585005,"d":"2.88"}},{"$f":"VLOOKUP(A20163,cordwood_density!A:D,4,FALSE)","v":1.1531},{"$f":"S20163/T20163","v":{"v":2.4987311174963187,"d":"2.50"}}]
["27063","27","MN","063","Jackson","","2104008610","Hydronic heater: outdoor","Hydronic heater",76.55159866157732,"A","CEC Survey",2017,15,"I",223.52750687552924,"TON",8,{"v":2.9199587047647366,"d":"2.92"},{"$f":"VLOOKUP(A20179,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2450858871019044,"d":"2.25"}]
["27065","27","MN","065","Kanabec","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",271.22253007730797,"A","CEC Survey",2017,15,"I",393.3330110142557,"TON",8,{"v":1.450222483,"d":"1.45"},{"$f":"VLOOKUP(A20202,cordwood_density!A:D,4,FALSE)","v":1.2997},{"v":1.1158132515195813,"d":"1.12"}]
["27067","27","MN","067","Kandiyohi","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",287.1812431908,"A","CEC Survey",2017,15,"I",403.88721064060053,"TON",8,{"v":1.4063843660300002,"d":"1.41"},{"$f":"VLOOKUP(A20219,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.08133505,"d":"1.08"}]
["27071","27","MN","071","Koochiching","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",186.01985296609,"A","CEC Survey",2017,15,"I",101.41614436649797,"TON",8,{"v":0.5451898963976999,"d":"0.55"},{"$f":"VLOOKUP(A20244,cordwood_density!A:D,4,FALSE)","v":1.1601},{"v":0.46995077699999993,"d":"0.47"}]
["27073","27","MN","073","Lac Qui Parle","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",20.18928312576,"A","CEC Survey",2017,15,"I",7.660562539913813,"TON",8,{"v":0.37943707521439995,"d":"0.38"},{"$f":"VLOOKUP(A20258,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.291740024,"d":"0.29"}]
["27079","27","MN","079","Le Sueur","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",167.17068241022992,"A","CEC Survey",2017,15,"I",481.2072232737051,"TON",8,{"v":2.8785383677075775,"d":"2.88"},{"$f":"VLOOKUP(A20297,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2132387880267395,"d":"2.21"}]
["27081","27","MN","081","Lincoln","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",49.1513864184,"A","CEC Survey",2017,15,"I",19.37457082105591,"TON",8,{"v":0.394181573153,"d":"0.39"},{"$f":"VLOOKUP(A20320,cordwood_density!A:D,4,FALSE)","v":1.349},{"v":0.292202797,"d":"0.29"}]
["27083","27","MN","083","Lyon","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1270.7335980199998,"A","CEC Survey",2017,15,"I",358.18816469790056,"TON",8,{"v":0.281875103685,"d":"0.28"},{"$f":"VLOOKUP(A20336,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.21672697500000002,"d":"0.22"}]
["27085","27","MN","085","McLeod","","2104009000","Wax Log; Total: All Combustor Types",null,1.8790989345952807,"A","CEC Survey",2017,15,"I",1.8377587580341845,"TON",8,{"v":0.978,"d":"0.98"},{"$f":"VLOOKUP(A20353,cordwood_density!A:D,4,FALSE)","v":1.3911},{"v":0.7030407591114944,"d":"0.70"}]
["27089","27","MN","089","Marshall","","2104008610","Hydronic heater: outdoor","Hydronic heater",138.77999190605976,"A","CEC Survey",2017,15,"I",438.21089035809894,"TON",8,{"v":3.157594148403785,"d":"3.16"},{"$f":"VLOOKUP(A20374,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.427798053516673,"d":"2.43"}]
["27091","27","MN","091","Martin","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",182.46626450280002,"A","CEC Survey",2017,15,"I",70.79600664823015,"TON",8,{"v":0.38799504577540006,"d":"0.39"},{"$f":"VLOOKUP(A20394,cordwood_density!A:D,4,FALSE)","v":1.3139},{"v":0.295300286,"d":"0.30"}]
["27093","27","MN","093","Meeker","","2104009000","Wax Log; Total: All Combustor Types",null,1.166670910340864,"A","CEC Survey",2017,15,"I",1.1410041503133648,"TON",8,{"v":0.9779999999999999,"d":"0.98"},{"$f":"VLOOKUP(A20413,cordwood_density!A:D,4,FALSE)","v":1.3139},{"v":0.7443488849988582,"d":"0.74"}]
["27099","27","MN","099","Mower","","2104008100","Fireplace: general","Fireplace: general",1307.021927644,"A","CEC Survey",2017,15,"I",475.4242813513708,"TON",8,{"v":0.3637462167206,"d":"0.36"},{"$f":"VLOOKUP(A20452,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.279675701,"d":"0.28"}]
["27101","27","MN","101","Murray","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",78.40663514354999,"A","CEC Survey",2017,15,"I",29.60464843933301,"TON",8,{"v":0.37757835653999994,"d":"0.38"},{"$f":"VLOOKUP(A20470,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.2903109,"d":"0.29"}]
["27103","27","MN","103","Nicollet","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",445.8788190129,"A","CEC Survey",2017,15,"I",594.1472135392195,"TON",8,{"v":1.33253069714,"d":"1.33"},{"$f":"VLOOKUP(A20491,cordwood_density!A:D,4,FALSE)","v":1.327},{"v":1.00416782,"d":"1.00"}]
["27107","27","MN","107","Norman","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.354261847882203,"A","CEC Survey",2017,15,"I",26.196151773391136,"TON",8,{"v":3.1356632399583972,"d":"3.14"},{"$f":"VLOOKUP(A20508,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.410935906472703,"d":"2.41"}]
["27109","27","MN","109","Olmsted","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2726.6810053723602,"A","CEC Survey",2017,15,"I",3467.93032546374,"TON",8,{"v":1.2718503993063,"d":"1.27"},{"$f":"VLOOKUP(A20535,cordwood_density!A:D,4,FALSE)","v":1.3541},{"v":0.939258843,"d":"0.94"}]
["27111","27","MN","111","Otter Tail","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1040.6160315,"A","CEC Survey",2017,15,"I",1022.2898351840803,"TON",8,{"$f":"P20547/J20547","v":{"v":0.982389089,"d":"0.98"}},{"$f":"VLOOKUP(A20547,cordwood_density!A:D,4,FALSE)","v":1.3587},{"$f":"S20547/T20547","v":{"v":0.7230360557886215,"d":"0.72"}}]
["27117","27","MN","117","Pipestone","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.713160785326234,"A","CEC Survey",2017,15,"I",4.991330851900031,"TON",8,{"v":2.913521541382668,"d":"2.91"},{"$f":"VLOOKUP(A20586,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.2401365072909947,"d":"2.24"}]
["27119","27","MN","119","Polk","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",760.3712566285499,"A","CEC Survey",2017,15,"I",1139.7805579089952,"TON",8,{"$f":"P20611/J20611","v":{"v":1.4989790158069995,"d":"1.50"}},{"$f":"VLOOKUP(A20611,cordwood_density!A:D,4,FALSE)","v":1.3006},{"$f":"S20611/T20611","v":{"v":1.1525288449999997,"d":"1.15"}}]
["27121","27","MN","121","Pope","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",553.19866637496,"A","CEC Survey",2017,15,"I",632.8386368893812,"TON",8,{"v":1.143962694336,"d":"1.14"},{"$f":"VLOOKUP(A20625,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":1.238054864,"d":"1.24"}]
["27125","27","MN","125","Red Lake","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",71.45468209882367,"A","CEC Survey",2017,15,"I",212.82369790181602,"TON",8,{"v":2.9784430026219324,"d":"2.98"},{"$f":"VLOOKUP(A20642,cordwood_density!A:D,4,FALSE)","v":1.2351},{"v":2.411499475849674,"d":"2.41"}]
["27127","27","MN","127","Redwood","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",168.98058639770002,"A","CEC Survey",2017,15,"I",68.03297705344711,"TON",8,{"v":0.4026082433714001,"d":"0.40"},{"$f":"VLOOKUP(A20664,cordwood_density!A:D,4,FALSE)","v":1.3733},{"v":0.2931684580000001,"d":"0.29"}]
["27129","27","MN","129","Renville","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,998.1641084309999,"A","CEC Survey",2017,15,"I",283.33827579735356,"TON",8,{"v":0.28385941089659994,"d":"0.28"},{"$f":"VLOOKUP(A20681,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.21825266099999996,"d":"0.22"}]
["27133","27","MN","133","Rock","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",62.40616062245007,"A","CEC Survey",2017,15,"I",180.51110343826642,"TON",8,{"v":2.8925205722931326,"d":"2.89"},{"$f":"VLOOKUP(A20702,cordwood_density!A:D,4,FALSE)","v":1.293},{"v":2.2370615408299557,"d":"2.24"}]
["27137","27","MN","137","St Louis","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1612.9317211118998,"A","CEC Survey",2017,15,"I",792.4112014228368,"TON",8,{"v":0.49128626528379993,"d":"0.49"},{"$f":"VLOOKUP(A20740,cordwood_density!A:D,4,FALSE)","v":1.0969},{"v":0.44788610199999995,"d":"0.45"}]
["27139","27","MN","139","Scott","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",531.60720990144,"A","CEC Survey",2017,15,"I",641.15515167505,"TON",8,{"v":1.2060693303875998,"d":"1.21"},{"$f":"VLOOKUP(A20759,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.9273176459999999,"d":"0.93"}]
["27143","27","MN","143","Sibley","","2104008620","Hydronic heater: indoor","Hydronic heater",90.7560579325086,"A","CEC Survey",2017,15,"I",267.4961964764946,"TON",8,{"v":2.947419737814308,"d":"2.95"},{"$f":"VLOOKUP(A20780,cordwood_density!A:D,4,FALSE)","v":1.2968},{"v":2.272840636809306,"d":"2.27"}]
["27145","27","MN","145","Stearns","","2104008100","Fireplace: general","Fireplace: general",4271.413884830001,"A","CEC Survey",2017,15,"I",1567.953631037441,"TON",8,{"v":0.3670807075395,"d":"0.37"},{"$f":"VLOOKUP(A20797,cordwood_density!A:D,4,FALSE)","v":1.3953},{"v":0.263083715,"d":"0.26"}]
["27147","27","MN","147","Steele","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",274.212653768,"A","CEC Survey",2017,15,"I",108.28528904770043,"TON",8,{"v":0.394895303188,"d":"0.39"},{"$f":"VLOOKUP(A20814,cordwood_density!A:D,4,FALSE)","v":1.3157},{"v":0.30014083999999996,"d":"0.30"}]
["27149","27","MN","149","Stevens","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",178.5581447265,"A","CEC Survey",2017,15,"I",255.89179165081885,"TON",8,{"v":1.43310064093,"d":"1.43"},{"$f":"VLOOKUP(A20836,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.10187655,"d":"1.10"}]
["27155","27","MN","155","Traverse","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",39.1709246964,"A","CEC Survey",2017,15,"I",14.65702955865961,"TON",8,{"v":0.37418135191499996,"d":"0.37"},{"$f":"VLOOKUP(A20875,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.287699025,"d":"0.29"}]
["27155","27","MN","155","Traverse","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",51.49681109855999,"A","CEC Survey",2017,15,"I",82.37533696359628,"TON",8,{"v":1.5996201552351996,"d":"1.60"},{"$f":"VLOOKUP(A20879,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.2299093919999997,"d":"1.23"}]
["27161","27","MN","161","Waseca","","2104008610","Hydronic heater: outdoor","Hydronic heater",94.54918421030915,"A","CEC Survey",2017,15,"I",271.8690342366726,"TON",8,{"v":2.8754244312880006,"d":"2.88"},{"$f":"VLOOKUP(A20914,cordwood_density!A:D,4,FALSE)","v":1.311},{"v":2.1933062023554544,"d":"2.19"}]
["27163","27","MN","163","Washington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",25.10475863588259,"A","CEC Survey",2017,15,"I",76.59638336852554,"TON",8,{"$f":"P20931/J20931","v":{"v":3.05107029625233,"d":"3.05"}},{"$f":"VLOOKUP(A20931,cordwood_density!A:D,4,FALSE)","v":1.4369},{"$f":"S20931/T20931","v":{"v":2.1233699605068757,"d":"2.12"}}]
["27165","27","MN","165","Watonwan","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",332.01404010247,"A","CEC Survey",2017,15,"I",482.9131908488869,"TON",8,{"v":1.4544962938912,"d":"1.45"},{"$f":"VLOOKUP(A20955,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.118327152,"d":"1.12"}]
["27167","27","MN","167","Wilkin","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",253.4780159644,"A","CEC Survey",2017,15,"I",363.2088307176843,"TON",8,{"v":1.4329007165998,"d":"1.43"},{"$f":"VLOOKUP(A20970,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.101722833,"d":"1.10"}]
["27171","27","MN","171","Wright","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",15.568111724854822,"A","CEC Survey",2017,15,"I",43.816933857508104,"TON",8,{"v":2.8145310511584674,"d":"2.81"},{"$f":"VLOOKUP(A20991,cordwood_density!A:D,4,FALSE)","v":1.2588},{"v":2.2358842160458114,"d":"2.24"}]
["28001","28","MS","001","Adams","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",254.69464601224,"A","CEC Survey",2017,15,"I",265.8149939143465,"TON",8,{"v":1.0436614906367998,"d":"1.04"},{"$f":"VLOOKUP(A21031,cordwood_density!A:D,4,FALSE)","v":1.2327},{"v":0.8466467839999999,"d":"0.85"}]
["28005","28","MS","005","Amite","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.6105037527324013,"A","CEC Survey",2017,15,"I",5.649095236257792,"TON",8,{"v":2.163986636810965,"d":"2.16"},{"$f":"VLOOKUP(A21048,cordwood_density!A:D,4,FALSE)","v":1.3104},{"v":1.651393953610321,"d":"1.65"}]
["28007","28","MS","007","Attala","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",253.79083943329644,"A","CEC Survey",2017,15,"I",212.8725668771259,"TON",8,{"v":0.8387716725807,"d":"0.84"},{"$f":"VLOOKUP(A21069,cordwood_density!A:D,4,FALSE)","v":1.2829},{"v":0.653809083,"d":"0.65"}]
["28009","28","MS","009","Benton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",108.13647240879999,"A","CEC Survey",2017,15,"I",81.82427964292611,"TON",8,{"v":0.7566760577652002,"d":"0.76"},{"$f":"VLOOKUP(A21084,cordwood_density!A:D,4,FALSE)","v":1.3358},{"v":0.566459094,"d":"0.57"}]
["28011","28","MS","011","Bolivar","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",283.44853916198997,"A","CEC Survey",2017,15,"I",297.75177775107227,"TON",8,{"v":1.0504615004592,"d":"1.05"},{"$f":"VLOOKUP(A21104,cordwood_density!A:D,4,FALSE)","v":1.2328},{"v":0.8520940140000001,"d":"0.85"}]
["28015","28","MS","015","Carroll","","2104008620","Hydronic heater: indoor","Hydronic heater",15.782741138200645,"A","CEC Survey",2017,15,"I",34.855834302547876,"TON",8,{"v":2.208477855483709,"d":"2.21"},{"$f":"VLOOKUP(A21125,cordwood_density!A:D,4,FALSE)","v":1.3198},{"v":1.6733428212484533,"d":"1.67"}]
["28019","28","MS","019","Choctaw","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",92.01662772120001,"A","CEC Survey",2017,15,"I",81.65511957833841,"TON",8,{"v":0.8873952632315999,"d":"0.89"},{"$f":"VLOOKUP(A21160,cordwood_density!A:D,4,FALSE)","v":1.2788},{"v":0.693928107,"d":"0.69"}]
["28023","28","MS","023","Clarke","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0930705901550097,"A","CEC Survey",2017,15,"I",2.3619086217004273,"TON",8,{"v":2.1608015465547217,"d":"2.16"},{"$f":"VLOOKUP(A21186,cordwood_density!A:D,4,FALSE)","v":1.3509},{"v":1.5995273865976176,"d":"1.60"}]
["28025","28","MS","025","Clay","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",174.82138193320003,"A","CEC Survey",2017,15,"I",112.94928413842369,"TON",8,{"v":0.6460839222835001,"d":"0.65"},{"$f":"VLOOKUP(A21203,cordwood_density!A:D,4,FALSE)","v":1.3399},{"v":0.48218816500000006,"d":"0.48"}]
["28027","28","MS","027","Coahoma","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",107.92372085739298,"A","CEC Survey",2017,15,"I",45.71490077662708,"TON",8,{"v":0.42358529166200004,"d":"0.42"},{"$f":"VLOOKUP(A21220,cordwood_density!A:D,4,FALSE)","v":1.2802},{"v":0.33087431,"d":"0.33"}]
["28031","28","MS","031","Covington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.1193789786821946,"A","CEC Survey",2017,15,"I",2.2422778501535894,"TON",8,{"v":2.0031445049944963,"d":"2.00"},{"$f":"VLOOKUP(A21246,cordwood_density!A:D,4,FALSE)","v":1.2568},{"v":1.5938450867238196,"d":"1.59"}]
["28033","28","MS","033","De Soto","","2104008610","Hydronic heater: outdoor","Hydronic heater",172.07650583505986,"A","CEC Survey",2017,15,"I",353.1476027879417,"TON",8,{"v":2.052270884245195,"d":"2.05"},{"$f":"VLOOKUP(A21259,cordwood_density!A:D,4,FALSE)","v":1.361},{"v":1.5079139487473878,"d":"1.51"}]
["28039","28","MS","039","George","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",38.128768861608954,"A","CEC Survey",2017,15,"I",73.88165023763035,"TON",8,{"v":1.9376877996189437,"d":"1.94"},{"$f":"VLOOKUP(A21302,cordwood_density!A:D,4,FALSE)","v":1.2204},{"v":1.5877481150597703,"d":"1.59"}]
["28041","28","MS","041","Greene","","2104008100","Fireplace: general","Fireplace: general",462.769347262,"A","CEC Survey",2017,15,"I",183.33390216443192,"TON",8,{"v":0.39616690960439993,"d":"0.40"},{"$f":"VLOOKUP(A21322,cordwood_density!A:D,4,FALSE)","v":1.3374},{"v":0.296221706,"d":"0.30"}]
["28043","28","MS","043","Grenada","","2104008100","Fireplace: general","Fireplace: general",1025.602692016,"A","CEC Survey",2017,15,"I",350.3967298755379,"TON",8,{"v":0.34164958087889996,"d":"0.34"},{"$f":"VLOOKUP(A21337,cordwood_density!A:D,4,FALSE)","v":1.3113},{"v":0.260542653,"d":"0.26"}]
["28045","28","MS","045","Hancock","","2104009000","Wax Log; Total: All Combustor Types",null,274.9791023220322,"A","CEC Survey",2017,15,"I",64.38148967859273,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A21358,cordwood_density!A:D,4,FALSE)","v":1.3085},{"v":0.17893183034008403,"d":"0.18"}]
["28047","28","MS","047","Harrison","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2060.6106749746,"A","CEC Survey",2017,15,"I",2003.8226564982583,"TON",8,{"v":0.9724411703938001,"d":"0.97"},{"$f":"VLOOKUP(A21375,cordwood_density!A:D,4,FALSE)","v":1.3562},{"v":0.717033749,"d":"0.72"}]
["28051","28","MS","051","Holmes","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.4843334704590343,"A","CEC Survey",2017,15,"I",5.322464378777331,"TON",8,{"v":2.1424114121820734,"d":"2.14"},{"$f":"VLOOKUP(A21393,cordwood_density!A:D,4,FALSE)","v":1.3441},{"v":1.5939375137133198,"d":"1.59"}]
["28055","28","MS","055","Issaquena","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",14.871880833040002,"A","CEC Survey",2017,15,"I",18.552774670116207,"TON",8,{"v":1.247506948072,"d":"1.25"},{"$f":"VLOOKUP(A21436,cordwood_density!A:D,4,FALSE)","v":1.226},{"v":1.017542372,"d":"1.02"}]
["28057","28","MS","057","Itawamba","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",341.78391068724005,"A","CEC Survey",2017,15,"I",446.5677910720921,"TON",8,{"v":1.30657932427,"d":"1.31"},{"$f":"VLOOKUP(A21451,cordwood_density!A:D,4,FALSE)","v":1.258},{"v":1.0386163149999998,"d":"1.04"}]
["28061","28","MS","061","Jasper","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",207.1598148313487,"A","CEC Survey",2017,15,"I",166.4327130718589,"TON",8,{"v":0.803402499695,"d":"0.80"},{"$f":"VLOOKUP(A21475,cordwood_density!A:D,4,FALSE)","v":1.2742},{"v":0.630515225,"d":"0.63"}]
["28063","28","MS","063","Jefferson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",84.635920325,"A","CEC Survey",2017,15,"I",30.906442319013635,"TON",8,{"v":0.36516933,"d":"0.37"},{"$f":"VLOOKUP(A21492,cordwood_density!A:D,4,FALSE)","v":1.2958},{"v":0.28180994752276584,"d":"0.28"}]
["28065","28","MS","065","Jefferson Davis","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",206.39060242102,"A","CEC Survey",2017,15,"I",160.95733117387158,"TON",8,{"v":0.7798675389566999,"d":"0.78"},{"$f":"VLOOKUP(A21504,cordwood_density!A:D,4,FALSE)","v":1.2953},{"v":0.602074839,"d":"0.60"}]
["28069","28","MS","069","Kemper","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7346903674727799,"A","CEC Survey",2017,15,"I",1.4820118695738191,"TON",8,{"v":2.017192459827272,"d":"2.02"},{"$f":"VLOOKUP(A21531,cordwood_density!A:D,4,FALSE)","v":1.226},{"v":1.645344583872163,"d":"1.65"}]
["28073","28","MS","073","Lamar","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",889.79677474688,"A","CEC Survey",2017,15,"I",972.3679514280701,"TON",8,{"v":1.0927977927372001,"d":"1.09"},{"$f":"VLOOKUP(A21570,cordwood_density!A:D,4,FALSE)","v":1.2276},{"v":0.890190447,"d":"0.89"}]
["28075","28","MS","075","Lauderdale","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",689.3867657107199,"A","CEC Survey",2017,15,"I",579.2761734664334,"TON",8,{"v":0.8402774788826001,"d":"0.84"},{"$f":"VLOOKUP(A21580,cordwood_density!A:D,4,FALSE)","v":1.3201},{"v":0.6365256260000001,"d":"0.64"}]
["28079","28","MS","079","Leake","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",346.0624444211391,"A","CEC Survey",2017,15,"I",285.1700839402896,"TON",8,{"v":0.8240422748480999,"d":"0.82"},{"$f":"VLOOKUP(A21609,cordwood_density!A:D,4,FALSE)","v":1.3131},{"v":0.627554851,"d":"0.63"}]
["28081","28","MS","081","Lee","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4403.91725426,"A","CEC Survey",2017,15,"I",1133.494827562465,"TON",8,{"v":0.25738331628870004,"d":"0.26"},{"$f":"VLOOKUP(A21626,cordwood_density!A:D,4,FALSE)","v":1.3161},{"v":0.195565167,"d":"0.20"}]
["28085","28","MS","085","Lincoln","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",60.019244448564834,"A","CEC Survey",2017,15,"I",122.78405843140108,"TON",8,{"v":2.045744820007261,"d":"2.05"},{"$f":"VLOOKUP(A21647,cordwood_density!A:D,4,FALSE)","v":1.2874},{"v":1.589051437010456,"d":"1.59"}]
["28087","28","MS","087","Lowndes","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.1153947414887404,"A","CEC Survey",2017,15,"I",4.364818188432695,"TON",8,{"v":2.0633587211060616,"d":"2.06"},{"$f":"VLOOKUP(A21666,cordwood_density!A:D,4,FALSE)","v":1.3279},{"v":1.5538509835876657,"d":"1.55"}]
["28091","28","MS","091","Marion","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",377.53012678801,"A","CEC Survey",2017,15,"I",471.32396033696125,"TON",8,{"v":1.2484406591519996,"d":"1.25"},{"$f":"VLOOKUP(A21704,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.9729119849999998,"d":"0.97"}]
["28095","28","MS","095","Monroe","","2104008620","Hydronic heater: indoor","Hydronic heater",43.0407052690791,"A","CEC Survey",2017,15,"I",84.27752623310522,"TON",8,{"v":1.9580888767092555,"d":"1.96"},{"$f":"VLOOKUP(A21725,cordwood_density!A:D,4,FALSE)","v":1.2228},{"v":1.601315731688956,"d":"1.60"}]
["28097","28","MS","097","Montgomery","","2104008100","Fireplace: general","Fireplace: general",734.1822485399999,"A","CEC Survey",2017,15,"I",266.0005899675471,"TON",8,{"v":0.3623086644992,"d":"0.36"},{"$f":"VLOOKUP(A21742,cordwood_density!A:D,4,FALSE)","v":1.3432},{"v":0.26973545600000004,"d":"0.27"}]
["28099","28","MS","099","Neshoba","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",452.68931114694,"A","CEC Survey",2017,15,"I",577.4025619075333,"TON",8,{"v":1.2754941362424,"d":"1.28"},{"$f":"VLOOKUP(A21764,cordwood_density!A:D,4,FALSE)","v":1.2888},{"v":0.989675773,"d":"0.99"}]
["28101","28","MS","101","Newton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",301.6349053956,"A","CEC Survey",2017,15,"I",397.29756702364966,"TON",8,{"v":1.3171471866048998,"d":"1.32"},{"$f":"VLOOKUP(A21781,cordwood_density!A:D,4,FALSE)","v":1.3027},{"v":1.011090187,"d":"1.01"}]
["28103","28","MS","103","Noxubee","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",182.37029749895999,"A","CEC Survey",2017,15,"I",244.9626739569558,"TON",8,{"v":1.3432158488328,"d":"1.34"},{"$f":"VLOOKUP(A21795,cordwood_density!A:D,4,FALSE)","v":1.3452},{"v":0.9985250140000002,"d":"1.00"}]
["28107","28","MS","107","Panola","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",267.78360001736,"A","CEC Survey",2017,15,"I",153.80783590656043,"TON",8,{"v":0.5743736207018999,"d":"0.57"},{"$f":"VLOOKUP(A21820,cordwood_density!A:D,4,FALSE)","v":1.3597},{"v":0.42242672699999995,"d":"0.42"}]
["28113","28","MS","113","Pike","","2104008610","Hydronic heater: outdoor","Hydronic heater",55.03794381180288,"A","CEC Survey",2017,15,"I",108.52041121556073,"TON",8,{"v":1.9717381082882774,"d":"1.97"},{"$f":"VLOOKUP(A21859,cordwood_density!A:D,4,FALSE)","v":1.2705},{"v":1.5519386920805018,"d":"1.55"}]
["28113","28","MS","113","Pike","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",422.936524598,"A","CEC Survey",2017,15,"I",500.645994779228,"TON",8,{"v":1.183737903117,"d":"1.18"},{"$f":"VLOOKUP(A21871,cordwood_density!A:D,4,FALSE)","v":1.2705},{"v":0.931710274,"d":"0.93"}]
["28117","28","MS","117","Prentiss","","2104009000","Wax Log; Total: All Combustor Types",null,136.9222137456753,"A","CEC Survey",2017,15,"I",47.02302471391008,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A21898,cordwood_density!A:D,4,FALSE)","v":1.3651},{"v":0.2515777232437184,"d":"0.25"}]
["28119","28","MS","119","Quitman","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",109.24186881023998,"A","CEC Survey",2017,15,"I",112.70697502098206,"TON",8,{"v":1.0317195801251,"d":"1.03"},{"$f":"VLOOKUP(A21915,cordwood_density!A:D,4,FALSE)","v":1.1989},{"v":0.8605551589999999,"d":"0.86"}]
["28123","28","MS","123","Scott","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.4640838547421704,"A","CEC Survey",2017,15,"I",3.1700318235492864,"TON",8,{"v":2.1651982659883497,"d":"2.17"},{"$f":"VLOOKUP(A21936,cordwood_density!A:D,4,FALSE)","v":1.3102},{"v":1.6525708029219583,"d":"1.65"}]
["28125","28","MS","125","Sharkey","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",44.67123069282,"A","CEC Survey",2017,15,"I",25.228397879590382,"TON",8,{"v":0.5647571711885999,"d":"0.56"},{"$f":"VLOOKUP(A21954,cordwood_density!A:D,4,FALSE)","v":1.4261},{"v":0.39601512599999994,"d":"0.40"}]
["28131","28","MS","131","Stone","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.525702451005228,"A","CEC Survey",2017,15,"I",5.158236004022707,"TON",8,{"v":2.042297580211688,"d":"2.04"},{"$f":"VLOOKUP(A21993,cordwood_density!A:D,4,FALSE)","v":1.3094},{"v":1.5597201620678847,"d":"1.56"}]
["28133","28","MS","133","Sunflower","","2104008100","Fireplace: general","Fireplace: general",757.16691246,"A","CEC Survey",2017,15,"I",328.46708402725415,"TON",8,{"v":0.43381066792800005,"d":"0.43"},{"$f":"VLOOKUP(A22012,cordwood_density!A:D,4,FALSE)","v":1.496},{"v":0.28998039300000006,"d":"0.29"}]
["28135","28","MS","135","Tallahatchie","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",161.57116380000002,"A","CEC Survey",2017,15,"I",39.696167506148804,"TON",8,{"v":0.24568844199999998,"d":"0.25"},{"$f":"VLOOKUP(A22032,cordwood_density!A:D,4,FALSE)","v":1.3489},{"v":0.1821398487656609,"d":"0.18"}]
["28139","28","MS","139","Tippah","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.2799708915790635,"A","CEC Survey",2017,15,"I",8.581982264909225,"TON",8,{"v":2.0051496802920936,"d":"2.01"},{"$f":"VLOOKUP(A22053,cordwood_density!A:D,4,FALSE)","v":1.2487},{"v":1.6057897655898885,"d":"1.61"}]
["28141","28","MS","141","Tishomingo","","2104008620","Hydronic heater: indoor","Hydronic heater",38.67167950459969,"A","CEC Survey",2017,15,"I",83.77977106604743,"TON",8,{"v":2.166437355173118,"d":"2.17"},{"$f":"VLOOKUP(A22070,cordwood_density!A:D,4,FALSE)","v":1.3209},{"v":1.6401221554796868,"d":"1.64"}]
["28143","28","MS","143","Tunica","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.27501368468546245,"A","CEC Survey",2017,15,"I",0.4612590088779593,"TON",8,{"v":1.6772220240803966,"d":"1.68"},{"$f":"VLOOKUP(A22086,cordwood_density!A:D,4,FALSE)","v":1.0469},{"v":1.6020842717359791,"d":"1.60"}]
["28145","28","MS","145","Union","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",331.06001486823,"A","CEC Survey",2017,15,"I",441.2617310742817,"TON",8,{"v":1.3328753436138,"d":"1.33"},{"$f":"VLOOKUP(A22109,cordwood_density!A:D,4,FALSE)","v":1.3434},{"v":0.9921656569999999,"d":"0.99"}]
["28151","28","MS","151","Washington","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",252.53583581919,"A","CEC Survey",2017,15,"I",94.88004991149663,"TON",8,{"v":0.3757092517334,"d":"0.38"},{"$f":"VLOOKUP(A22148,cordwood_density!A:D,4,FALSE)","v":1.1414},{"v":0.329165281,"d":"0.33"}]
["28153","28","MS","153","Wayne","","2104008100","Fireplace: general","Fireplace: general",882.239026124,"A","CEC Survey",2017,15,"I",311.9041981475797,"TON",8,{"v":0.35353706752,"d":"0.35"},{"$f":"VLOOKUP(A22162,cordwood_density!A:D,4,FALSE)","v":1.28},{"v":0.276200834,"d":"0.28"}]
["28157","28","MS","157","Wilkinson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",17.065564952300324,"A","CEC Survey",2017,15,"I",34.44059607754663,"TON",8,{"v":2.018133954182646,"d":"2.02"},{"$f":"VLOOKUP(A22187,cordwood_density!A:D,4,FALSE)","v":1.2211},{"v":1.6527180035890965,"d":"1.65"}]
["28159","28","MS","159","Winston","","2104008610","Hydronic heater: outdoor","Hydronic heater",46.510307763526356,"A","CEC Survey",2017,15,"I",99.70733394012888,"TON",8,{"v":2.1437685264753275,"d":"2.14"},{"$f":"VLOOKUP(A22204,cordwood_density!A:D,4,FALSE)","v":1.3351},{"v":1.6056988438883435,"d":"1.61"}]
["28161","28","MS","161","Yalobusha","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",185.717240208,"A","CEC Survey",2017,15,"I",71.92774892399628,"TON",8,{"v":0.387297102,"d":"0.39"},{"$f":"VLOOKUP(A22227,cordwood_density!A:D,4,FALSE)","v":1.3532},{"v":0.2862083224948271,"d":"0.29"}]
["28163","28","MS","163","Yazoo","","2104009000","Wax Log; Total: All Combustor Types",null,124.12480555063996,"A","CEC Survey",2017,15,"I",29.061626210624098,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A22243,cordwood_density!A:D,4,FALSE)","v":1.3177},{"v":0.17768255293314106,"d":"0.18"}]
["29005","29","MO","005","Atchison","","2104008100","Fireplace: general","Fireplace: general",157.767381156,"A","CEC Survey",2017,15,"I",180.01658808320278,"TON",8,{"v":1.1410253929816,"d":"1.14"},{"$f":"VLOOKUP(A22282,cordwood_density!A:D,4,FALSE)","v":1.2796},{"v":0.891704746,"d":"0.89"}]
["29007","29","MO","007","Audrain","","2104009000","Wax Log; Total: All Combustor Types",null,151.70749515048277,"A","CEC Survey",2017,15,"I",21.23904932106759,"TON",8,0.14,{"$f":"VLOOKUP(A22303,cordwood_density!A:D,4,FALSE)","v":1.3735},{"v":0.10192937750273026,"d":"0.10"}]
["29009","29","MO","009","Barry","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",675.6913163409499,"A","CEC Survey",2017,15,"I",2599.488628198692,"TON",8,{"v":3.8471541151004005,"d":"3.85"},{"$f":"VLOOKUP(A22321,cordwood_density!A:D,4,FALSE)","v":1.4326},{"v":2.685434954,"d":"2.69"}]
["29013","29","MO","013","Bates","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.122931874164813,"A","CEC Survey",2017,15,"I",26.188128516205627,"TON",8,{"v":6.351821789805971,"d":"6.35"},{"$f":"VLOOKUP(A22338,cordwood_density!A:D,4,FALSE)","v":1.3362},{"v":4.7536460034470664,"d":"4.75"}]
["29015","29","MO","015","Benton","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.089376267405459,"A","CEC Survey",2017,15,"I",14.940563833104898,"TON",8,{"v":7.15072917510342,"d":"7.15"},{"$f":"VLOOKUP(A22356,cordwood_density!A:D,4,FALSE)","v":1.4179},{"v":5.043182999579251,"d":"5.04"}]
["29017","29","MO","017","Bollinger","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",223.614633525,"A","CEC Survey",2017,15,"I",322.6479319232625,"TON",8,{"v":1.442874855,"d":"1.44"},{"$f":"VLOOKUP(A22377,cordwood_density!A:D,4,FALSE)","v":1.4726},{"v":0.979814515143284,"d":"0.98"}]
["29021","29","MO","021","Buchanan","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.312356942784751,"A","CEC Survey",2017,15,"I",67.81879135100903,"TON",8,{"v":5.995107093421872,"d":"6.00"},{"$f":"VLOOKUP(A22398,cordwood_density!A:D,4,FALSE)","v":1.2914},{"v":4.642331650473805,"d":"4.64"}]
["29025","29","MO","025","Caldwell","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",178.370962302,"A","CEC Survey",2017,15,"I",224.96559443464014,"TON",8,{"v":1.261223192,"d":"1.26"},{"$f":"VLOOKUP(A22437,cordwood_density!A:D,4,FALSE)","v":1.2857},{"v":0.980962271136346,"d":"0.98"}]
["29027","29","MO","027","Callaway","","2104009000","Wax Log; Total: All Combustor Types",null,258.35351690795443,"A","CEC Survey",2017,15,"I",36.16949236711363,"TON",8,0.14,{"$f":"VLOOKUP(A22453,cordwood_density!A:D,4,FALSE)","v":1.3904},{"v":0.10069044879171461,"d":"0.10"}]
["29031","29","MO","031","Cape Girardeau","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.370810253350445,"A","CEC Survey",2017,15,"I",21.631991694812925,"TON",8,{"v":6.417445678916998,"d":"6.42"},{"$f":"VLOOKUP(A22476,cordwood_density!A:D,4,FALSE)","v":1.4055},{"v":4.565952101684097,"d":"4.57"}]
["29033","29","MO","033","Carroll","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",24.454187465480963,"A","CEC Survey",2017,15,"I",24.21137638321397,"TON",8,{"v":0.9900707769330002,"d":"0.99"},{"$f":"VLOOKUP(A22493,cordwood_density!A:D,4,FALSE)","v":1.2215},{"v":0.8105368620000001,"d":"0.81"}]
["29037","29","MO","037","Cass","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.970152052069217,"A","CEC Survey",2017,15,"I",78.17083653477599,"TON",8,{"v":5.595560896074682,"d":"5.60"},{"$f":"VLOOKUP(A22518,cordwood_density!A:D,4,FALSE)","v":1.2345},{"v":4.53265362176969,"d":"4.53"}]
["29039","29","MO","039","Cedar","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",48.921281790617634,"A","CEC Survey",2017,15,"I",338.4822796600261,"TON",8,{"v":6.918916824557567,"d":"6.92"},{"$f":"VLOOKUP(A22532,cordwood_density!A:D,4,FALSE)","v":1.4208},{"v":4.869733125392432,"d":"4.87"}]
["29043","29","MO","043","Christian","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4664.979175098,"A","CEC Survey",2017,15,"I",3512.925316192471,"TON",8,{"v":0.7530420146235,"d":"0.75"},{"$f":"VLOOKUP(A22571,cordwood_density!A:D,4,FALSE)","v":1.4195},{"v":0.530498073,"d":"0.53"}]
["29047","29","MO","047","Clay","","2104008610","Hydronic heater: outdoor","Hydronic heater",327.7896129162048,"A","CEC Survey",2017,15,"I",1911.008564318496,"TON",8,{"v":5.8299851155046225,"d":"5.83"},{"$f":"VLOOKUP(A22594,cordwood_density!A:D,4,FALSE)","v":1.3291},{"v":4.386415706496594,"d":"4.39"}]
["29049","29","MO","049","Clinton","","2104008620","Hydronic heater: indoor","Hydronic heater",47.98344396098759,"A","CEC Survey",2017,15,"I",305.9745881425423,"TON",8,{"v":6.376670011250371,"d":"6.38"},{"$f":"VLOOKUP(A22610,cordwood_density!A:D,4,FALSE)","v":1.3187},{"v":4.83557292124848,"d":"4.84"}]
["29051","29","MO","051","Cole","","2104008100","Fireplace: general","Fireplace: general",2543.099256402,"A","CEC Survey",2017,15,"I",2365.9516383611603,"TON",8,{"v":0.9303418387642999,"d":"0.93"},{"$f":"VLOOKUP(A22627,cordwood_density!A:D,4,FALSE)","v":1.4039},{"v":0.662683837,"d":"0.66"}]
["29053","29","MO","053","Cooper","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",247.32715783858458,"A","CEC Survey",2017,15,"I",193.02961693813904,"TON",8,{"v":0.780462682,"d":"0.78"},{"$f":"VLOOKUP(A22647,cordwood_density!A:D,4,FALSE)","v":1.4419},{"v":0.5412737929121298,"d":"0.54"}]
["29055","29","MO","055","Crawford","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",539.9337470849,"A","CEC Survey",2017,15,"I",2115.7994436782938,"TON",8,{"v":3.918627896666,"d":"3.92"},{"$f":"VLOOKUP(A22666,cordwood_density!A:D,4,FALSE)","v":1.4191},{"v":2.76134726,"d":"2.76"}]
["29059","29","MO","059","Dallas","","2104008100","Fireplace: general","Fireplace: general",361.93449730920617,"A","CEC Survey",2017,15,"I",409.33484262814454,"TON",8,{"v":1.1309638779153002,"d":"1.13"},{"$f":"VLOOKUP(A22687,cordwood_density!A:D,4,FALSE)","v":1.4337},{"v":0.7888427690000002,"d":"0.79"}]
["29063","29","MO","063","Dekalb","","2104009000","Wax Log; Total: All Combustor Types",null,61.82517566987,"A","CEC Survey",2017,15,"I",8.6555245937818,"TON",8,{"$f":"P22723/J22723","v":0.14},{"$f":"VLOOKUP(A22723,cordwood_density!A:D,4,FALSE)","v":1.3642},{"$f":"S22723/T22723","v":{"v":0.10262424864389386,"d":"0.10"}}]
["29067","29","MO","067","Douglas","","2104008610","Hydronic heater: outdoor","Hydronic heater",50.73591103182401,"A","CEC Survey",2017,15,"I",360.6015117124818,"TON",8,{"v":7.107421634476912,"d":"7.11"},{"$f":"VLOOKUP(A22744,cordwood_density!A:D,4,FALSE)","v":1.4535},{"v":4.889866965584391,"d":"4.89"}]
["29069","29","MO","069","Dunklin","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",228.00388148999997,"A","CEC Survey",2017,15,"I",227.43132221714046,"TON",8,{"v":0.9974888178696001,"d":"1.00"},{"$f":"VLOOKUP(A22765,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.766945116,"d":"0.77"}]
["29071","29","MO","071","Franklin","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.571382142299013,"A","CEC Survey",2017,15,"I",75.0161058151566,"TON",8,{"v":7.0961492835451,"d":"7.10"},{"$f":"VLOOKUP(A22776,cordwood_density!A:D,4,FALSE)","v":1.404},{"v":5.0542373814423796,"d":"5.05"}]
["29073","29","MO","073","Gasconade","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",609.41105789895,"A","CEC Survey",2017,15,"I",2421.2018000211174,"TON",8,{"v":3.9730191446945993,"d":"3.97"},{"$f":"VLOOKUP(A22800,cordwood_density!A:D,4,FALSE)","v":1.4079},{"v":2.821946974,"d":"2.82"}]
["29077","29","MO","077","Greene","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",9.757801901859002,"A","CEC Survey",2017,15,"I",59.170578247162325,"TON",8,{"v":6.063924933328424,"d":"6.06"},{"$f":"VLOOKUP(A22821,cordwood_density!A:D,4,FALSE)","v":1.4142},{"v":4.287883561963247,"d":"4.29"}]
["29081","29","MO","081","Harrison","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",265.97747754144,"A","CEC Survey",2017,15,"I",959.1685801552818,"TON",8,{"v":3.6062022582563995,"d":"3.61"},{"$f":"VLOOKUP(A22860,cordwood_density!A:D,4,FALSE)","v":1.3794},{"v":2.6143267059999995,"d":"2.61"}]
["29085","29","MO","085","Hickory","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",127.99633875875,"A","CEC Survey",2017,15,"I",196.48261989200265,"TON",8,{"v":1.5350643760392,"d":"1.54"},{"$f":"VLOOKUP(A22885,cordwood_density!A:D,4,FALSE)","v":1.4631},{"v":1.049186232,"d":"1.05"}]
["29087","29","MO","087","Holt","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",63.520734127500006,"A","CEC Survey",2017,15,"I",51.43297081796197,"TON",8,{"v":0.8097036585680001,"d":"0.81"},{"$f":"VLOOKUP(A22899,cordwood_density!A:D,4,FALSE)","v":1.036},{"v":0.781567238,"d":"0.78"}]
["29089","29","MO","089","Howard","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,551.493096725,"A","CEC Survey",2017,15,"I",425.53791667090604,"TON",8,{"v":0.7716105953055999,"d":"0.77"},{"$f":"VLOOKUP(A22916,cordwood_density!A:D,4,FALSE)","v":1.4576},{"v":0.529370606,"d":"0.53"}]
["29093","29","MO","093","Iron","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.491830251789057,"A","CEC Survey",2017,15,"I",23.65415672132853,"TON",8,{"v":6.774142789217547,"d":"6.77"},{"$f":"VLOOKUP(A22938,cordwood_density!A:D,4,FALSE)","v":1.3717},{"v":4.938501705341946,"d":"4.94"}]
["29095","29","MO","095","Jackson","","2104008620","Hydronic heater: indoor","Hydronic heater",594.9452616223217,"A","CEC Survey",2017,15,"I",2061.2073361463877,"TON",8,{"v":3.4645327378955857,"d":"3.46"},{"$f":"VLOOKUP(A22955,cordwood_density!A:D,4,FALSE)","v":1.2725},{"v":2.72261904746215,"d":"2.72"}]
["29101","29","MO","101","Johnson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.374047422803748,"A","CEC Survey",2017,15,"I",52.959538558983,"TON",8,{"v":6.32424631543959,"d":"6.32"},{"$f":"VLOOKUP(A22998,cordwood_density!A:D,4,FALSE)","v":1.342},{"v":4.712553141162138,"d":"4.71"}]
["29103","29","MO","103","Knox","","2104008610","Hydronic heater: outdoor","Hydronic heater",16.664663644166097,"A","CEC Survey",2017,15,"I",117.77002062956886,"TON",8,{"v":7.067050565451847,"d":"7.07"},{"$f":"VLOOKUP(A23014,cordwood_density!A:D,4,FALSE)","v":1.4311},{"v":4.9381947910361585,"d":"4.94"}]
["29105","29","MO","105","Laclede","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",130.29930498899998,"A","CEC Survey",2017,15,"I",211.75900095797098,"TON",8,{"v":1.6251736797510004,"d":"1.63"},{"$f":"VLOOKUP(A23033,cordwood_density!A:D,4,FALSE)","v":1.4345},{"v":1.1329199580000002,"d":"1.13"}]
["29107","29","MO","107","Lafayette","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",185.00602870944,"A","CEC Survey",2017,15,"I",591.7906750330053,"TON",8,{"v":3.198764273581799,"d":"3.20"},{"$f":"VLOOKUP(A23054,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":2.5135661429999994,"d":"2.51"}]
["29109","29","MO","109","Lawrence","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",558.977394836,"A","CEC Survey",2017,15,"I",402.65436743527056,"TON",8,{"v":0.720341057,"d":"0.72"},{"$f":"VLOOKUP(A23067,cordwood_density!A:D,4,FALSE)","v":1.3972},{"v":0.5155604473232178,"d":"0.52"}]
["29113","29","MO","113","Lincoln","","2104008610","Hydronic heater: outdoor","Hydronic heater",179.42796801678023,"A","CEC Survey",2017,15,"I",1274.8105061040612,"TON",8,{"v":7.1048595165768145,"d":"7.10"},{"$f":"VLOOKUP(A23089,cordwood_density!A:D,4,FALSE)","v":1.4084},{"v":5.044631863516624,"d":"5.04"}]
["29119","29","MO","119","Mcdonald","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",79.82926899149965,"A","CEC Survey",2017,15,"I",567.5970409269029,"TON",8,{"v":7.110137022391394,"d":"7.11"},{"$f":"VLOOKUP(A23132,cordwood_density!A:D,4,FALSE)","v":1.4465},{"v":4.9154075509100545,"d":"4.92"}]
["29119","29","MO","119","Mcdonald","","2104009000","Wax Log; Total: All Combustor Types",null,130.5322922744505,"A","CEC Survey",2017,15,"I",18.27452091842307,"TON",8,0.14,{"$f":"VLOOKUP(A23143,cordwood_density!A:D,4,FALSE)","v":1.4465},{"v":0.09678534393363292,"d":"0.10"}]
["29123","29","MO","123","Madison","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,781.5463593730001,"A","CEC Survey",2017,15,"I",615.1139202803018,"TON",8,{"$f":"P23171/J23171","v":{"v":0.7870472594534,"d":"0.79"}},{"$f":"VLOOKUP(A23171,cordwood_density!A:D,4,FALSE)","v":1.4762},{"$f":"S23171/T23171","v":{"v":0.533157607,"d":"0.53"}}]
["29125","29","MO","125","Maries","","2104009000","Wax Log; Total: All Combustor Types",null,58.825355278473914,"A","CEC Survey",2017,15,"I",8.235549738986348,"TON",8,0.14,{"$f":"VLOOKUP(A23188,cordwood_density!A:D,4,FALSE)","v":1.4246},{"v":0.09827319949459498,"d":"0.10"}]
["29129","29","MO","129","Mercer","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",28.859632417199997,"A","CEC Survey",2017,15,"I",98.67122363340744,"TON",8,{"v":3.4190048648922002,"d":"3.42"},{"$f":"VLOOKUP(A23219,cordwood_density!A:D,4,FALSE)","v":1.2261},{"v":2.788520402,"d":"2.79"}]
["29131","29","MO","131","Miller","","2104008100","Fireplace: general","Fireplace: general",663.69164515,"A","CEC Survey",2017,15,"I",701.7393180757949,"TON",8,{"v":1.057327334469,"d":"1.06"},{"$f":"VLOOKUP(A23227,cordwood_density!A:D,4,FALSE)","v":1.4178},{"v":0.745752105,"d":"0.75"}]
["29135","29","MO","135","Moniteau","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",215.7708166992,"A","CEC Survey",2017,15,"I",701.6237310772966,"TON",8,{"v":3.2517081865404,"d":"3.25"},{"$f":"VLOOKUP(A23266,cordwood_density!A:D,4,FALSE)","v":1.3116},{"v":2.4791919689999995,"d":"2.48"}]
["29139","29","MO","139","Montgomery","","2104008100","Fireplace: general","Fireplace: general",353.760744708,"A","CEC Survey",2017,15,"I",396.8667076232481,"TON",8,{"v":1.12185061107,"d":"1.12"},{"$f":"VLOOKUP(A23287,cordwood_density!A:D,4,FALSE)","v":1.421},{"v":0.78947967,"d":"0.79"}]
["29141","29","MO","141","Morgan","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",230.8633367768,"A","CEC Survey",2017,15,"I",368.47242244667257,"TON",8,{"v":1.5960629677760996,"d":"1.60"},{"$f":"VLOOKUP(A23305,cordwood_density!A:D,4,FALSE)","v":1.4111},{"v":1.1310771509999997,"d":"1.13"}]
["29143","29","MO","143","New Madrid","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",258.676115359,"A","CEC Survey",2017,15,"I",133.2280334997626,"TON",8,{"v":0.515038017,"d":"0.52"},{"$f":"VLOOKUP(A23322,cordwood_density!A:D,4,FALSE)","v":1.3696},{"v":0.3760499540011682,"d":"0.38"}]
["29147","29","MO","147","Nodaway","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.27096453354168,"A","CEC Survey",2017,15,"I",27.2440048191215,"TON",8,{"v":6.3788880954554585,"d":"6.38"},{"$f":"VLOOKUP(A23343,cordwood_density!A:D,4,FALSE)","v":1.3077},{"v":4.877944555674435,"d":"4.88"}]
["29149","29","MO","149","Oregon","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.968014688173116,"A","CEC Survey",2017,15,"I",29.457468249063496,"TON",8,{"v":7.423729639122326,"d":"7.42"},{"$f":"VLOOKUP(A23358,cordwood_density!A:D,4,FALSE)","v":1.4841},{"v":5.002176160044692,"d":"5.00"}]
["29153","29","MO","153","Ozark","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",425.35637827899996,"A","CEC Survey",2017,15,"I",1839.7838387272245,"TON",8,{"v":4.32527624523,"d":"4.33"},{"$f":"VLOOKUP(A23400,cordwood_density!A:D,4,FALSE)","v":1.4782},{"v":2.9260426500000003,"d":"2.93"}]
["29157","29","MO","157","Perry","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.3942373087784743,"A","CEC Survey",2017,15,"I",9.311121953026943,"TON",8,{"v":6.6782906284330075,"d":"6.68"},{"$f":"VLOOKUP(A23421,cordwood_density!A:D,4,FALSE)","v":1.4271},{"v":4.679623452058726,"d":"4.68"}]
["29159","29","MO","159","Pettis","","2104008610","Hydronic heater: outdoor","Hydronic heater",74.62070076547163,"A","CEC Survey",2017,15,"I",471.97294429490654,"TON",8,{"v":6.324959956866247,"d":"6.32"},{"$f":"VLOOKUP(A23434,cordwood_density!A:D,4,FALSE)","v":1.3704},{"v":4.6154115271937,"d":"4.62"}]
["29161","29","MO","161","Phelps","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1126.9268209127001,"A","CEC Survey",2017,15,"I",4080.149879239462,"TON",8,{"v":3.6205987855848005,"d":"3.62"},{"$f":"VLOOKUP(A23460,cordwood_density!A:D,4,FALSE)","v":1.3918},{"v":2.6013786360000006,"d":"2.60"}]
["29165","29","MO","165","Platte","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",154.4837580344894,"A","CEC Survey",2017,15,"I",918.9138295083229,"TON",8,{"v":5.9482876465445,"d":"5.95"},{"$f":"VLOOKUP(A23477,cordwood_density!A:D,4,FALSE)","v":1.2614},{"v":4.71562362973244,"d":"4.72"}]
["29169","29","MO","169","Pulaski","","2104008620","Hydronic heater: indoor","Hydronic heater",70.88068552884512,"A","CEC Survey",2017,15,"I",497.1404773931631,"TON",8,{"v":7.0137650854244376,"d":"7.01"},{"$f":"VLOOKUP(A23510,cordwood_density!A:D,4,FALSE)","v":1.4438},{"v":4.8578508695279385,"d":"4.86"}]
["29169","29","MO","169","Pulaski","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2024.9823330000002,"A","CEC Survey",2017,15,"I",1508.104368273166,"TON",8,{"v":0.7447493954374,"d":"0.74"},{"$f":"VLOOKUP(A23516,cordwood_density!A:D,4,FALSE)","v":1.4438},{"v":0.515825873,"d":"0.52"}]
["29175","29","MO","175","Randolph","","2104008620","Hydronic heater: indoor","Hydronic heater",34.10130860674913,"A","CEC Survey",2017,15,"I",225.133652893946,"TON",8,{"$f":"P23555/J23555","v":{"v":6.601906557022533,"d":"6.60"}},{"$f":"VLOOKUP(A23555,cordwood_density!A:D,4,FALSE)","v":1.3901},{"$f":"S23555/T23555","v":{"v":4.749231391283025,"d":"4.75"}}]
["29175","29","MO","175","Randolph","","2104009000","Wax Log; Total: All Combustor Types",null,133.91711637054354,"A","CEC Survey",2017,15,"I",18.748396291876098,"TON",8,0.14,{"$f":"VLOOKUP(A23563,cordwood_density!A:D,4,FALSE)","v":1.3901},{"v":0.10071217897992953,"d":"0.10"}]
["29179","29","MO","179","Reynolds","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",68.31752510736,"A","CEC Survey",2017,15,"I",306.7440969080286,"TON",8,{"v":4.4899767142616,"d":"4.49"},{"$f":"VLOOKUP(A23594,cordwood_density!A:D,4,FALSE)","v":1.4684},{"v":3.057734074,"d":"3.06"}]
["29181","29","MO","181","Ripley","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",351.0483086334,"A","CEC Survey",2017,15,"I",1547.9993600112264,"TON",8,{"v":4.409647680791999,"d":"4.41"},{"$f":"VLOOKUP(A23611,cordwood_density!A:D,4,FALSE)","v":1.466},{"v":3.0079452119999996,"d":"3.01"}]
["29185","29","MO","185","St Clair","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.603683010814678,"A","CEC Survey",2017,15,"I",24.01386616526775,"TON",8,{"v":6.66370102287076,"d":"6.66"},{"$f":"VLOOKUP(A23628,cordwood_density!A:D,4,FALSE)","v":1.323},{"v":5.036811052812366,"d":"5.04"}]
["29186","29","MO","186","Ste Genevieve","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",214.12753235119797,"A","CEC Survey",2017,15,"I",384.16297372174637,"TON",8,{"v":1.7940849058666,"d":"1.79"},{"$f":"VLOOKUP(A23650,cordwood_density!A:D,4,FALSE)","v":1.4174},{"v":1.265757659,"d":"1.27"}]
["29195","29","MO","195","Saline","","2104008610","Hydronic heater: outdoor","Hydronic heater",56.01324324582714,"A","CEC Survey",2017,15,"I",372.0287798062978,"TON",8,{"v":6.641800371629313,"d":"6.64"},{"$f":"VLOOKUP(A23689,cordwood_density!A:D,4,FALSE)","v":1.3947},{"v":4.762171342675352,"d":"4.76"}]
["29197","29","MO","197","Schuyler","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",36.735228419399995,"A","CEC Survey",2017,15,"I",43.3039646979507,"TON",8,{"v":1.1788129967114,"d":"1.18"},{"$f":"VLOOKUP(A23710,cordwood_density!A:D,4,FALSE)","v":1.3946},{"v":0.845269609,"d":"0.85"}]
["29199","29","MO","199","Scotland","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",38.11475514,"A","CEC Survey",2017,15,"I",41.75576151853141,"TON",8,{"v":1.095527476568,"d":"1.10"},{"$f":"VLOOKUP(A23725,cordwood_density!A:D,4,FALSE)","v":1.3846},{"v":0.7912230800000001,"d":"0.79"}]
["29203","29","MO","203","Shannon","","2104008610","Hydronic heater: outdoor","Hydronic heater",41.93336550483719,"A","CEC Survey",2017,15,"I",315.8613602506557,"TON",8,{"v":7.532459091894729,"d":"7.53"},{"$f":"VLOOKUP(A23749,cordwood_density!A:D,4,FALSE)","v":1.4672},{"v":5.133900689677432,"d":"5.13"}]
["29205","29","MO","205","Shelby","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7257243388526858,"A","CEC Survey",2017,15,"I",5.200049428983248,"TON",8,{"v":7.1653231820833305,"d":"7.17"},{"$f":"VLOOKUP(A23766,cordwood_density!A:D,4,FALSE)","v":1.4415},{"v":4.970741021216323,"d":"4.97"}]
["29209","29","MO","209","Stone","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1899.67771728,"A","CEC Survey",2017,15,"I",1466.5488733894892,"TON",8,{"v":0.7719987764500001,"d":"0.77"},{"$f":"VLOOKUP(A23801,cordwood_density!A:D,4,FALSE)","v":1.4575},{"v":0.5296732600000001,"d":"0.53"}]
["29209","29","MO","209","Stone","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1130.8414294744,"A","CEC Survey",2017,15,"I",4565.129138497198,"TON",8,{"v":4.036931279232499,"d":"4.04"},{"$f":"VLOOKUP(A23805,cordwood_density!A:D,4,FALSE)","v":1.4575},{"v":2.7697641709999994,"d":"2.77"}]
["29215","29","MO","215","Texas","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",465.99279244686,"A","CEC Survey",2017,15,"I",862.270384244491,"TON",8,{"v":1.8503942512004001,"d":"1.85"},{"$f":"VLOOKUP(A23844,cordwood_density!A:D,4,FALSE)","v":1.4746},{"v":1.2548448740000002,"d":"1.25"}]
["29217","29","MO","217","Vernon","","2104008610","Hydronic heater: outdoor","Hydronic heater",52.396324285274915,"A","CEC Survey",2017,15,"I",350.87401611656657,"TON",8,{"v":6.696538753486066,"d":"6.70"},{"$f":"VLOOKUP(A23854,cordwood_density!A:D,4,FALSE)","v":1.407},{"v":4.759444743060459,"d":"4.76"}]
["29221","29","MO","221","Washington","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.4851109015261015,"A","CEC Survey",2017,15,"I",55.72796874579824,"TON",8,{"v":7.445176094109193,"d":"7.45"},{"$f":"VLOOKUP(A23883,cordwood_density!A:D,4,FALSE)","v":1.4603},{"v":5.098388066910356,"d":"5.10"}]
["29223","29","MO","223","Wayne","","2104008620","Hydronic heater: indoor","Hydronic heater",42.606695115871936,"A","CEC Survey",2017,15,"I",316.67335342285827,"TON",8,{"v":7.432478688188384,"d":"7.43"},{"$f":"VLOOKUP(A23900,cordwood_density!A:D,4,FALSE)","v":1.4535},{"v":5.113504429438173,"d":"5.11"}]
["29225","29","MO","225","Webster","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",537.6131014502699,"A","CEC Survey",2017,15,"I",820.3356711161714,"TON",8,{"v":1.525884821079,"d":"1.53"},{"$f":"VLOOKUP(A23919,cordwood_density!A:D,4,FALSE)","v":1.4667},{"v":1.04035237,"d":"1.04"}]
["29227","29","MO","227","Worth","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",17.942618407679998,"A","CEC Survey",2017,15,"I",61.55243022296344,"TON",8,{"$f":"P23939/J23939","v":{"v":3.43051548132,"d":"3.43"}},{"$f":"VLOOKUP(A23939,cordwood_density!A:D,4,FALSE)","v":1.24},{"$f":"S23939/T23939","v":{"v":2.766544743,"d":"2.77"}}]
["30001","30","MT","001","Beaverhead","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",69.3374260995,"A","CEC Survey",2017,15,"I",20.939879265344114,"TON",8,{"v":0.30199966227899994,"d":"0.30"},{"$f":"VLOOKUP(A23978,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.29695148699999996,"d":"0.30"}]
["30003","30","MT","003","Big Horn","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",58.2707359864,"A","CEC Survey",2017,15,"I",15.341476347746593,"TON",8,{"v":0.26327926167480004,"d":"0.26"},{"$f":"VLOOKUP(A23995,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.256207923,"d":"0.26"}]
["30007","30","MT","007","Broadwater","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",69.26944266307918,"A","CEC Survey",2017,15,"I",142.7908761502804,"TON",8,{"v":2.061383355497797,"d":"2.06"},{"$f":"VLOOKUP(A24017,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.0269256199585026,"d":"2.03"}]
["30009","30","MT","009","Carbon","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",69.00725238605,"A","CEC Survey",2017,15,"I",18.772642801620954,"TON",8,{"v":0.272038693797,"d":"0.27"},{"$f":"VLOOKUP(A24038,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.26749134100000005,"d":"0.27"}]
["30011","30","MT","011","Carter","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.260478940984647,"A","CEC Survey",2017,15,"I",2.569255651066405,"TON",8,{"v":2.0383169980288462,"d":"2.04"},{"$f":"VLOOKUP(A24048,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.004244835819908,"d":"2.00"}]
["30013","30","MT","013","Cascade","","2104009000","Wax Log; Total: All Combustor Types",null,651.0889958607545,"A","CEC Survey",2017,15,"I",508.171315170942,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A24073,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["30017","30","MT","017","Custer","","2104008610","Hydronic heater: outdoor","Hydronic heater",40.834622246338185,"A","CEC Survey",2017,15,"I",79.84684746156856,"TON",8,{"v":1.9553712773412215,"d":"1.96"},{"$f":"VLOOKUP(A24094,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.902852547042839,"d":"1.90"}]
["30021","30","MT","021","Dawson","","2104009000","Wax Log; Total: All Combustor Types",null,76.59759149163109,"A","CEC Survey",2017,15,"I",59.78399121270571,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A24133,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["30023","30","MT","023","Deer Lodge","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",55.324623795840004,"A","CEC Survey",2017,15,"I",20.59062991935017,"TON",8,{"v":0.37217839917600004,"d":"0.37"},{"$f":"VLOOKUP(A24145,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.3659571280000001,"d":"0.37"}]
["30027","30","MT","027","Fergus","","2104008100","Fireplace: general","Fireplace: general",377.04949261012547,"A","CEC Survey",2017,15,"I",94.77960676885219,"TON",8,{"v":0.25137179236799995,"d":"0.25"},{"$f":"VLOOKUP(A24172,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.24716990399999997,"d":"0.25"}]
["30029","30","MT","029","Flathead","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",950.93830486954,"A","CEC Survey",2017,15,"I",432.2298497196025,"TON",8,{"v":0.45452985488779996,"d":"0.45"},{"$f":"VLOOKUP(A24189,cordwood_density!A:D,4,FALSE)","v":1.0037},{"v":0.45285429399999994,"d":"0.45"}]
["30031","30","MT","031","Gallatin","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1941.6817741689,"A","CEC Survey",2017,15,"I",1924.7002404880484,"TON",8,{"v":0.991254213792,"d":"0.99"},{"$f":"VLOOKUP(A24210,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.974684576,"d":"0.97"}]
["30035","30","MT","035","Glacier","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.442575892554805,"A","CEC Survey",2017,15,"I",11.076786996444978,"TON",8,{"v":2.035210388448146,"d":"2.04"},{"$f":"VLOOKUP(A24228,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.0011901557995535,"d":"2.00"}]
["30039","30","MT","039","Granite","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",64.132043822,"A","CEC Survey",2017,15,"I",70.32374965670006,"TON",8,{"v":1.096546211,"d":"1.10"},{"$f":"VLOOKUP(A24267,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.0782165299901671,"d":"1.08"}]
["30041","30","MT","041","Hill","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",212.26894262784003,"A","CEC Survey",2017,15,"I",205.7076595443569,"TON",8,{"v":0.9690897641348,"d":"0.97"},{"$f":"VLOOKUP(A24286,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9430612729999999,"d":"0.94"}]
["30045","30","MT","045","Judith Basin","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7865224890218094,"A","CEC Survey",2017,15,"I",1.6253654204048502,"TON",8,{"v":2.066521228688962,"d":"2.07"},{"$f":"VLOOKUP(A24306,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.031977609330346,"d":"2.03"}]
["30047","30","MT","047","Lake","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",306.60684913488,"A","CEC Survey",2017,15,"I",113.26747217088315,"TON",8,{"$f":"P24323/J24323","v":{"v":0.3694225112402999,"d":"0.37"}},{"$f":"VLOOKUP(A24323,cordwood_density!A:D,4,FALSE)","v":1.0171},{"$f":"S24323/T24323","v":{"v":0.36321159299999994,"d":"0.36"}}]
["30049","30","MT","049","Lewis and Clark","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",493.3257635958599,"A","CEC Survey",2017,15,"I",171.3111424144789,"TON",8,{"v":0.34725764404799997,"d":"0.35"},{"$f":"VLOOKUP(A24339,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.341452944,"d":"0.34"}]
["30053","30","MT","053","Lincoln","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",273.0834566617195,"A","CEC Survey",2017,15,"I",592.3586326207783,"TON",8,{"v":2.169148727872443,"d":"2.17"},{"$f":"VLOOKUP(A24362,cordwood_density!A:D,4,FALSE)","v":1.0056},{"v":2.157069140684609,"d":"2.16"}]
["30055","30","MT","055","McCone","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",15.7602363696,"A","CEC Survey",2017,15,"I",3.906972389289726,"TON",8,{"v":0.24790062139080002,"d":"0.25"},{"$f":"VLOOKUP(A24383,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.241242333,"d":"0.24"}]
["30059","30","MT","059","Meagher","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",18.255103236720004,"A","CEC Survey",2017,15,"I",5.818287569598573,"TON",8,{"v":0.3187211539782,"d":"0.32"},{"$f":"VLOOKUP(A24415,cordwood_density!A:D,4,FALSE)","v":0.9942},{"v":0.320580521,"d":"0.32"}]
["30063","30","MT","063","Missoula","","2104008620","Hydronic heater: indoor","Hydronic heater",313.5001520704053,"A","CEC Survey",2017,15,"I",620.6153110550752,"TON",8,{"v":1.9796332057781538,"d":"1.98"},{"$f":"VLOOKUP(A24440,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.946541991915589,"d":"1.95"}]
["30065","30","MT","065","Musselshell","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,311.750644425,"A","CEC Survey",2017,15,"I",60.285205044460106,"TON",8,{"v":0.19337636063480002,"d":"0.19"},{"$f":"VLOOKUP(A24461,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.188182523,"d":"0.19"}]
["30069","30","MT","069","Petroleum","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,32.74405432,"A","CEC Survey",2017,15,"I",6.371872040422269,"TON",8,{"v":0.19459630680280002,"d":"0.19"},{"$f":"VLOOKUP(A24491,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.189369703,"d":"0.19"}]
["30071","30","MT","071","Phillips","","2104008620","Hydronic heater: indoor","Hydronic heater",27.16888709577487,"A","CEC Survey",2017,15,"I",55.460785984897115,"TON",8,{"v":2.0413344790086017,"d":"2.04"},{"$f":"VLOOKUP(A24500,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.986506888875634,"d":"1.99"}]
["30073","30","MT","073","Pondera","","2104008100","Fireplace: general","Fireplace: general",163.533610216,"A","CEC Survey",2017,15,"I",41.65583625623804,"TON",8,{"v":0.25472339417699996,"d":"0.25"},{"$f":"VLOOKUP(A24517,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.250465481,"d":"0.25"}]
["30077","30","MT","077","Powell","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",108.50362454400002,"A","CEC Survey",2017,15,"I",111.23226967625182,"TON",8,{"v":1.025147962971,"d":"1.03"},{"$f":"VLOOKUP(A24556,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.0080117630000003,"d":"1.01"}]
["30081","30","MT","081","Ravalli","","2104008100","Fireplace: general","Fireplace: general",1425.314893296,"A","CEC Survey",2017,15,"I",381.8867829032863,"TON",8,{"v":0.2679315179399999,"d":"0.27"},{"$f":"VLOOKUP(A24577,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.2634528199999999,"d":"0.26"}]
["30083","30","MT","083","Richland","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",50.23774854476,"A","CEC Survey",2017,15,"I",12.285059087313487,"TON",8,{"v":0.24453840873000005,"d":"0.24"},{"$f":"VLOOKUP(A24595,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.23797042500000004,"d":"0.24"}]
["30085","30","MT","085","Roosevelt","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",123.950920749,"A","CEC Survey",2017,15,"I",80.10069964475468,"TON",8,{"v":0.646229162,"d":"0.65"},{"$f":"VLOOKUP(A24612,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.6288722868820552,"d":"0.63"}]
["30087","30","MT","087","Rosebud","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",282.27729858460003,"A","CEC Survey",2017,15,"I",311.94884652087626,"TON",8,{"v":1.105114892643,"d":"1.11"},{"$f":"VLOOKUP(A24630,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.086641979,"d":"1.09"}]
["30091","30","MT","091","Sheridan","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.6802265469139233,"A","CEC Survey",2017,15,"I",3.5363511607093834,"TON",8,{"v":2.1046871132970786,"d":"2.10"},{"$f":"VLOOKUP(A24651,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.0481579537729453,"d":"2.05"}]
["30097","30","MT","097","Sweet Grass","","2104008610","Hydronic heater: outdoor","Hydronic heater",33.027942969706416,"A","CEC Survey",2017,15,"I",65.72746574312288,"TON",8,{"v":1.9900562927400236,"d":"1.99"},{"$f":"VLOOKUP(A24694,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9567908483186074,"d":"1.96"}]
["30097","30","MT","097","Sweet Grass","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",82.75308852048,"A","CEC Survey",2017,15,"I",90.97026863761154,"TON",8,{"v":1.099297564164,"d":"1.10"},{"$f":"VLOOKUP(A24706,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.080921892,"d":"1.08"}]
["30101","30","MT","101","Toole","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",32.83840345606,"A","CEC Survey",2017,15,"I",8.218304273500626,"TON",8,{"v":0.2502650375344,"d":"0.25"},{"$f":"VLOOKUP(A24729,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24354324399999996,"d":"0.24"}]
["30103","30","MT","103","Treasure","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",37.20529715405,"A","CEC Survey",2017,15,"I",41.355543037634725,"TON",8,{"v":1.1115498652355997,"d":"1.11"},{"$f":"VLOOKUP(A24750,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.0816950809999997,"d":"1.08"}]
["30109","30","MT","109","Wibaux","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",11.875812317816624,"A","CEC Survey",2017,15,"I",23.796717612384185,"TON",8,{"v":2.0037970435658776,"d":"2.00"},{"$f":"VLOOKUP(A24782,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.949977660145852,"d":"1.95"}]
["30109","30","MT","109","Wibaux","","2104008620","Hydronic heater: indoor","Hydronic heater",7.382261711075199,"A","CEC Survey",2017,15,"I",14.792554191482063,"TON",8,{"v":2.0037970435658776,"d":"2.00"},{"$f":"VLOOKUP(A24785,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.949977660145852,"d":"1.95"}]
["31003","31","NE","003","Antelope","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.853313884717923,"A","CEC Survey",2017,15,"I",7.683315760608451,"TON",8,{"v":1.9939501401845696,"d":"1.99"},{"$f":"VLOOKUP(A24828,cordwood_density!A:D,4,FALSE)","v":1.1931},{"v":1.6712347164400045,"d":"1.67"}]
["31003","31","NE","003","Antelope","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",52.0385198592,"A","CEC Survey",2017,15,"I",14.442332061042931,"TON",8,{"$f":"P24835/J24835","v":{"v":0.27753156892469993,"d":"0.28"}},{"$f":"VLOOKUP(A24835,cordwood_density!A:D,4,FALSE)","v":1.1931},{"$f":"S24835/T24835","v":{"v":0.23261383699999993,"d":"0.23"}}]
["31007","31","NE","007","Banner","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",16.3815108,"A","CEC Survey",2017,15,"I",8.247242191066604,"TON",8,{"v":0.503448204,"d":"0.50"},{"$f":"VLOOKUP(A24867,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.40600661612903227,"d":"0.41"}]
["31009","31","NE","009","Blaine","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",6.61424415456,"A","CEC Survey",2017,15,"I",8.088922814226926,"TON",8,{"v":1.2229549779546998,"d":"1.22"},{"$f":"VLOOKUP(A24884,cordwood_density!A:D,4,FALSE)","v":1.3471},{"v":0.9078427569999998,"d":"0.91"}]
["31013","31","NE","013","Box Butte","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,580.38148661,"A","CEC Survey",2017,15,"I",107.7402649097167,"TON",8,{"v":0.185636977394,"d":"0.19"},{"$f":"VLOOKUP(A24911,cordwood_density!A:D,4,FALSE)","v":1.094},{"v":0.169686451,"d":"0.17"}]
["31015","31","NE","015","Boyd","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",8.0141129994,"A","CEC Survey",2017,15,"I",2.3694286010882832,"TON",8,{"v":0.29565699925440003,"d":"0.30"},{"$f":"VLOOKUP(A24923,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":0.23156093300000002,"d":"0.23"}]
["31021","31","NE","021","Burt","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",46.900301677531154,"A","CEC Survey",2017,15,"I",97.11676472835353,"TON",8,{"v":2.0707066107184535,"d":"2.07"},{"$f":"VLOOKUP(A24962,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":1.669924686063269,"d":"1.67"}]
["31023","31","NE","023","Butler","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",24.04332372,"A","CEC Survey",2017,15,"I",5.335813859369415,"TON",8,{"v":0.2219249685072,"d":"0.22"},{"$f":"VLOOKUP(A24983,cordwood_density!A:D,4,FALSE)","v":0.9492},{"v":0.233802116,"d":"0.23"}]
["31025","31","NE","025","Cass","","2104008100","Fireplace: general","Fireplace: general",680.2435176900001,"A","CEC Survey",2017,15,"I",213.88107554598463,"TON",8,{"v":0.314418395742,"d":"0.31"},{"$f":"VLOOKUP(A24997,cordwood_density!A:D,4,FALSE)","v":1.2426},{"v":0.25303267,"d":"0.25"}]
["31027","31","NE","027","Cedar","","2104009000","Wax Log; Total: All Combustor Types",null,56.27470582509184,"A","CEC Survey",2017,15,"I",43.922092758131555,"TON",8,{"v":0.7804943999999998,"d":"0.78"},{"$f":"VLOOKUP(A25018,cordwood_density!A:D,4,FALSE)","v":1.2069},{"v":0.6466935123042503,"d":"0.65"}]
["31031","31","NE","031","Cherry","","2104008610","Hydronic heater: outdoor","Hydronic heater",34.15687505147595,"A","CEC Survey",2017,15,"I",70.3765336149718,"TON",8,{"v":2.060391458788639,"d":"2.06"},{"$f":"VLOOKUP(A25039,cordwood_density!A:D,4,FALSE)","v":1.2252},{"v":1.6816776516394376,"d":"1.68"}]
["31035","31","NE","035","Clay","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",14.90965614144,"A","CEC Survey",2017,15,"I",3.9749881083481435,"TON",8,{"v":0.26660494854070005,"d":"0.27"},{"$f":"VLOOKUP(A25073,cordwood_density!A:D,4,FALSE)","v":1.1627},{"v":0.22929814100000004,"d":"0.23"}]
["31037","31","NE","037","Colfax","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",187.22398182074997,"A","CEC Survey",2017,15,"I",181.3829269914667,"TON",8,{"v":0.9688017807736,"d":"0.97"},{"$f":"VLOOKUP(A25096,cordwood_density!A:D,4,FALSE)","v":1.2062},{"v":0.803185028,"d":"0.80"}]
["31041","31","NE","041","Custer","","2104008100","Fireplace: general","Fireplace: general",267.9246878319109,"A","CEC Survey",2017,15,"I",89.75866929193315,"TON",8,{"v":0.3350145521052,"d":"0.34"},{"$f":"VLOOKUP(A25117,cordwood_density!A:D,4,FALSE)","v":1.3266},{"v":0.252536222,"d":"0.25"}]
["31041","31","NE","041","Custer","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",273.7008927531162,"A","CEC Survey",2017,15,"I",303.47670705081026,"TON",8,{"v":1.1087896133556001,"d":"1.11"},{"$f":"VLOOKUP(A25126,cordwood_density!A:D,4,FALSE)","v":1.3266},{"v":0.835813066,"d":"0.84"}]
["31045","31","NE","045","Dawes","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",151.30897839768835,"A","CEC Survey",2017,15,"I",154.4751043327573,"TON",8,{"v":1.0209249045800002,"d":"1.02"},{"$f":"VLOOKUP(A25156,cordwood_density!A:D,4,FALSE)","v":1.2712},{"v":0.8031190250000001,"d":"0.80"}]
["31049","31","NE","049","Deuel","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.912884782296254,"A","CEC Survey",2017,15,"I",1.8935084507444122,"TON",8,{"v":2.0742031058744512,"d":"2.07"},{"$f":"VLOOKUP(A25173,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.5948047869248434,"d":"1.59"}]
["31053","31","NE","053","Dodge","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",91.78019065860461,"A","CEC Survey",2017,15,"I",169.1764655802935,"TON",8,{"v":1.843278646146861,"d":"1.84"},{"$f":"VLOOKUP(A25202,cordwood_density!A:D,4,FALSE)","v":1.1644},{"v":1.583028723932378,"d":"1.58"}]
["31053","31","NE","053","Dodge","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",461.66294694,"A","CEC Survey",2017,15,"I",120.99892821824976,"TON",8,{"v":0.262093653,"d":"0.26"},{"$f":"VLOOKUP(A25212,cordwood_density!A:D,4,FALSE)","v":1.1644},{"v":0.22508901837856404,"d":"0.23"}]
["31059","31","NE","059","Fillmore","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.7912086603231938,"A","CEC Survey",2017,15,"I",1.6206719343371987,"TON",8,{"v":2.0483495891907766,"d":"2.05"},{"$f":"VLOOKUP(A25251,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.5749266409278615,"d":"1.57"}]
["31061","31","NE","061","Franklin","","2104008100","Fireplace: general","Fireplace: general",103.98636947799999,"A","CEC Survey",2017,15,"I",33.81157367828012,"TON",8,{"v":0.32515390092,"d":"0.33"},{"$f":"VLOOKUP(A25267,cordwood_density!A:D,4,FALSE)","v":1.16},{"v":0.280305087,"d":"0.28"}]
["31063","31","NE","063","Frontier","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",100.00332318585001,"A","CEC Survey",2017,15,"I",109.38552712496275,"TON",8,{"v":1.0938189216139997,"d":"1.09"},{"$f":"VLOOKUP(A25290,cordwood_density!A:D,4,FALSE)","v":1.234},{"v":0.8864010709999998,"d":"0.89"}]
["31067","31","NE","067","Gage","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",68.94019063733226,"A","CEC Survey",2017,15,"I",150.85374234719708,"TON",8,{"v":2.18818284302085,"d":"2.19"},{"$f":"VLOOKUP(A25307,cordwood_density!A:D,4,FALSE)","v":1.4015},{"v":1.561314907613878,"d":"1.56"}]
["31067","31","NE","067","Gage","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",563.00169290565,"A","CEC Survey",2017,15,"I",608.173213766115,"TON",8,{"v":1.0802333659555001,"d":"1.08"},{"$f":"VLOOKUP(A25320,cordwood_density!A:D,4,FALSE)","v":1.4015},{"v":0.7707694370000001,"d":"0.77"}]
["31071","31","NE","071","Garfield","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,142.393384654,"A","CEC Survey",2017,15,"I",29.923291935925775,"TON",8,{"v":0.2101452396025,"d":"0.21"},{"$f":"VLOOKUP(A25346,cordwood_density!A:D,4,FALSE)","v":1.2325},{"v":0.170503237,"d":"0.17"}]
["31077","31","NE","077","Greeley","","2104008620","Hydronic heater: indoor","Hydronic heater",9.946198570170036,"A","CEC Survey",2017,15,"I",21.364917598008446,"TON",8,{"v":2.148048568232355,"d":"2.15"},{"$f":"VLOOKUP(A25385,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.6515827835094228,"d":"1.65"}]
["31079","31","NE","079","Hall","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2745.9094920320003,"A","CEC Survey",2017,15,"I",548.3375413947196,"TON",8,{"v":0.19969250369900005,"d":"0.20"},{"$f":"VLOOKUP(A25406,cordwood_density!A:D,4,FALSE)","v":1.193},{"v":0.16738684300000004,"d":"0.17"}]
["31081","31","NE","081","Hamilton","","2104008100","Fireplace: general","Fireplace: general",276.955330144,"A","CEC Survey",2017,15,"I",71.34006970259759,"TON",8,{"v":0.2575869172314,"d":"0.26"},{"$f":"VLOOKUP(A25417,cordwood_density!A:D,4,FALSE)","v":1.0653},{"v":0.241797538,"d":"0.24"}]
["31085","31","NE","085","Hayes","","2104008620","Hydronic heater: indoor","Hydronic heater",4.5959002315832445,"A","CEC Survey",2017,15,"I",9.926032079578992,"TON",8,{"v":2.1597579537011766,"d":"2.16"},{"$f":"VLOOKUP(A25445,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.6605858478403634,"d":"1.66"}]
["31087","31","NE","087","Hitchcock","","2104008100","Fireplace: general","Fireplace: general",41.89820189900001,"A","CEC Survey",2017,15,"I",15.137647826860249,"TON",8,{"v":0.3612958824188,"d":"0.36"},{"$f":"VLOOKUP(A25462,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.27779169800000003,"d":"0.28"}]
["31091","31","NE","091","Hooker","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",2.7939842784,"A","CEC Survey",2017,15,"I",0.6857084317593232,"TON",8,{"v":0.24542315325839995,"d":"0.25"},{"$f":"VLOOKUP(A25493,cordwood_density!A:D,4,FALSE)","v":1.1292},{"v":0.21734250199999997,"d":"0.22"}]
["31091","31","NE","091","Hooker","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",26.336427026,"A","CEC Survey",2017,15,"I",27.179779405820753,"TON",8,{"v":1.0320222776988,"d":"1.03"},{"$f":"VLOOKUP(A25501,cordwood_density!A:D,4,FALSE)","v":1.1292},{"v":0.9139410889999999,"d":"0.91"}]
["31097","31","NE","097","Johnson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",35.65145693865,"A","CEC Survey",2017,15,"I",11.268608432961186,"TON",8,{"v":0.3160770807306,"d":"0.32"},{"$f":"VLOOKUP(A25540,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.243024051,"d":"0.24"}]
["31097","31","NE","097","Johnson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",107.6166708708,"A","CEC Survey",2017,15,"I",123.56348512608945,"TON",8,{"v":1.1481816351151999,"d":"1.15"},{"$f":"VLOOKUP(A25546,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.882809192,"d":"0.88"}]
["31103","31","NE","103","Keya Paha","","2104008610","Hydronic heater: outdoor","Hydronic heater",6.9808232435699376,"A","CEC Survey",2017,15,"I",11.025248459136483,"TON",8,{"v":1.5793622148063813,"d":"1.58"},{"$f":"VLOOKUP(A25579,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":1.7092664662406722,"d":"1.71"}]
["31105","31","NE","105","Kimball","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.5295152217109662,"A","CEC Survey",2017,15,"I",1.0450879183520028,"TON",8,{"v":1.9736692648326923,"d":"1.97"},{"$f":"VLOOKUP(A25596,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":1.5916687619618486,"d":"1.59"}]
["31107","31","NE","107","Knox","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.8113464165217132,"A","CEC Survey",2017,15,"I",3.798997909405064,"TON",8,{"v":2.0973337152703193,"d":"2.10"},{"$f":"VLOOKUP(A25611,cordwood_density!A:D,4,FALSE)","v":1.2325},{"v":1.7016906411929569,"d":"1.70"}]
["31109","31","NE","109","Lancaster","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",4333.64023274684,"A","CEC Survey",2017,15,"I",3504.624479833227,"TON",8,{"v":0.8087022206759998,"d":"0.81"},{"$f":"VLOOKUP(A25635,cordwood_density!A:D,4,FALSE)","v":1.2504},{"v":0.6467548149999999,"d":"0.65"}]
["31115","31","NE","115","Loup","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",9.9851827061,"A","CEC Survey",2017,15,"I",2.8115600350404084,"TON",8,{"v":0.28157321881780006,"d":"0.28"},{"$f":"VLOOKUP(A25674,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.21649486300000007,"d":"0.22"}]
["31117","31","NE","117","McPherson","","2104008100","Fireplace: general","Fireplace: general",6.771013824,"A","CEC Survey",2017,15,"I",2.4276973546844727,"TON",8,{"v":0.3585426669902,"d":"0.36"},{"$f":"VLOOKUP(A25687,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.275674817,"d":"0.28"}]
["31121","31","NE","121","Merrick","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.62550217453105,"A","CEC Survey",2017,15,"I",5.530390471993325,"TON",8,{"v":2.1064124515460083,"d":"2.11"},{"$f":"VLOOKUP(A25713,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.6195697766769248,"d":"1.62"}]
["31123","31","NE","123","Morrill","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",53.16820118425,"A","CEC Survey",2017,15,"I",11.170316362712455,"TON",8,{"v":0.210093930468,"d":"0.21"},{"$f":"VLOOKUP(A25734,cordwood_density!A:D,4,FALSE)","v":0.9483},{"v":0.22154796000000002,"d":"0.22"}]
["31127","31","NE","127","Nemaha","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",17.530755133429835,"A","CEC Survey",2017,15,"I",4.881051559329756,"TON",8,{"v":0.27842791267,"d":"0.28"},{"$f":"VLOOKUP(A25763,cordwood_density!A:D,4,FALSE)","v":1.1356},{"v":0.245181325,"d":"0.25"}]
["31127","31","NE","127","Nemaha","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",42.60269112625954,"A","CEC Survey",2017,15,"I",38.088127968135545,"TON",8,{"v":0.8940310332803999,"d":"0.89"},{"$f":"VLOOKUP(A25769,cordwood_density!A:D,4,FALSE)","v":1.1356},{"v":0.7872763589999999,"d":"0.79"}]
["31131","31","NE","131","Otoe","","2104008620","Hydronic heater: indoor","Hydronic heater",33.535815485233314,"A","CEC Survey",2017,15,"I",65.51830139168646,"TON",8,{"v":1.9536814728878702,"d":"1.95"},{"$f":"VLOOKUP(A25790,cordwood_density!A:D,4,FALSE)","v":1.2492},{"v":1.5639461038167388,"d":"1.56"}]
["31135","31","NE","135","Perkins","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",25.827902008560002,"A","CEC Survey",2017,15,"I",29.318843652413786,"TON",8,{"v":1.1351616419597998,"d":"1.14"},{"$f":"VLOOKUP(A25829,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.8727984329999999,"d":"0.87"}]
["31137","31","NE","137","Phelps","","2104008100","Fireplace: general","Fireplace: general",290.52981648,"A","CEC Survey",2017,15,"I",69.00123724481588,"TON",8,{"v":0.23750139686459998,"d":"0.24"},{"$f":"VLOOKUP(A25837,cordwood_density!A:D,4,FALSE)","v":1.0042},{"v":0.236508063,"d":"0.24"}]
["31141","31","NE","141","Platte","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",80.00007571764,"A","CEC Survey",2017,15,"I",23.21444860436998,"TON",8,{"v":0.29018033290749995,"d":"0.29"},{"$f":"VLOOKUP(A25868,cordwood_density!A:D,4,FALSE)","v":1.2479},{"v":0.23253492499999995,"d":"0.23"}]
["31143","31","NE","143","Polk","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",38.236725400299996,"A","CEC Survey",2017,15,"I",10.618192889089755,"TON",8,{"v":0.2776961881,"d":"0.28"},{"$f":"VLOOKUP(A25885,cordwood_density!A:D,4,FALSE)","v":1.2125},{"v":0.22902778400000004,"d":"0.23"}]
["31145","31","NE","145","Red Willow","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",149.269421422,"A","CEC Survey",2017,15,"I",34.6035429357737,"TON",8,{"v":0.23181936800000003,"d":"0.23"},{"$f":"VLOOKUP(A25902,cordwood_density!A:D,4,FALSE)","v":1.2239},{"v":0.18941038320124196,"d":"0.19"}]
["31149","31","NE","149","Rock","","2104008610","Hydronic heater: outdoor","Hydronic heater",10.856105652813298,"A","CEC Survey",2017,15,"I",23.662765166730953,"TON",8,{"v":2.17967344123985,"d":"2.18"},{"$f":"VLOOKUP(A25924,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.6758983863138937,"d":"1.68"}]
["31153","31","NE","153","Sarpy","","2104009000","Wax Log; Total: All Combustor Types",null,1024.286271846619,"A","CEC Survey",2017,15,"I",799.4496991731637,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A25963,cordwood_density!A:D,4,FALSE)","v":1.2081},{"v":0.6460511547057363,"d":"0.65"}]
["31155","31","NE","155","Saunders","","2104009000","Wax Log; Total: All Combustor Types",null,130.7408359391387,"A","CEC Survey",2017,15,"I",102.04249030181649,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A25978,cordwood_density!A:D,4,FALSE)","v":1.3192},{"v":0.5916422073984232,"d":"0.59"}]
["31159","31","NE","159","Seward","","2104008100","Fireplace: general","Fireplace: general",418.811904896,"A","CEC Survey",2017,15,"I",125.63299717075834,"TON",8,{"v":0.2999747516775,"d":"0.30"},{"$f":"VLOOKUP(A26002,cordwood_density!A:D,4,FALSE)","v":1.2175},{"v":0.24638583299999997,"d":"0.25"}]
["31161","31","NE","161","Sheridan","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",62.326419608900004,"A","CEC Survey",2017,15,"I",18.16718288356157,"TON",8,{"v":0.29148446192739996,"d":"0.29"},{"$f":"VLOOKUP(A26019,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.22411537899999998,"d":"0.22"}]
["31165","31","NE","165","Sioux","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",16.14337284384,"A","CEC Survey",2017,15,"I",18.971125865075916,"TON",8,{"v":1.1751649453054,"d":"1.18"},{"$f":"VLOOKUP(A26054,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.9035560090000001,"d":"0.90"}]
["31167","31","NE","167","Stanton","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.8444250202369075,"A","CEC Survey",2017,15,"I",5.32541828442194,"TON",8,{"v":1.8722301507453323,"d":"1.87"},{"$f":"VLOOKUP(A26058,cordwood_density!A:D,4,FALSE)","v":1.1136},{"v":1.6812411554825184,"d":"1.68"}]
["31169","31","NE","169","Thayer","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",65.32692220764001,"A","CEC Survey",2017,15,"I",19.084906352953663,"TON",8,{"v":0.29214458156,"d":"0.29"},{"$f":"VLOOKUP(A26079,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.235600469,"d":"0.24"}]
["31173","31","NE","173","Thurston","","2104008100","Fireplace: general","Fireplace: general",129.96754218,"A","CEC Survey",2017,15,"I",44.523643419696484,"TON",8,{"v":0.34257509738880004,"d":"0.34"},{"$f":"VLOOKUP(A26107,cordwood_density!A:D,4,FALSE)","v":1.2858},{"v":0.266429536,"d":"0.27"}]
["31177","31","NE","177","Washington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.292360522251235,"A","CEC Survey",2017,15,"I",4.225551932273982,"TON",8,{"v":1.8433190989191512,"d":"1.84"},{"$f":"VLOOKUP(A26136,cordwood_density!A:D,4,FALSE)","v":1.1333},{"v":1.6265058668659236,"d":"1.63"}]
["31179","31","NE","179","Wayne","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",127.47872058799999,"A","CEC Survey",2017,15,"I",47.21328742715723,"TON",8,{"v":0.370362106,"d":"0.37"},{"$f":"VLOOKUP(A26157,cordwood_density!A:D,4,FALSE)","v":1.2858},{"v":0.28804021309690464,"d":"0.29"}]
["31183","31","NE","183","Wheeler","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",3.3682766544,"A","CEC Survey",2017,15,"I",0.9403255349692976,"TON",8,{"v":0.279171110764,"d":"0.28"},{"$f":"VLOOKUP(A26183,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.21464793999999998,"d":"0.21"}]
["31185","31","NE","185","York","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2073147765419747,"A","CEC Survey",2017,15,"I",2.5053131093507157,"TON",8,{"v":2.07511177534537,"d":"2.08"},{"$f":"VLOOKUP(A26196,cordwood_density!A:D,4,FALSE)","v":1.2926},{"v":1.605378133487057,"d":"1.61"}]
["32001","32","NV","001","Churchill","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",120.93042307574,"A","CEC Survey",2017,15,"I",28.784860621320963,"TON",8,{"v":0.23802828014000002,"d":"0.24"},{"$f":"VLOOKUP(A26213,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.23163515,"d":"0.23"}]
["32007","32","NV","007","Elko","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",133.386151223613,"A","CEC Survey",2017,15,"I",236.40197859318377,"TON",8,{"v":1.7723127657898425,"d":"1.77"},{"$f":"VLOOKUP(A26252,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7247107491142881,"d":"1.72"}]
["32009","32","NV","009","Esmeralda","","2104008610","Hydronic heater: outdoor","Hydronic heater",2.832243460198876,"A","CEC Survey",2017,15,"I",4.971863155789357,"TON",8,{"v":1.755450484980638,"d":"1.76"},{"$f":"VLOOKUP(A26269,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7083013672446847,"d":"1.71"}]
["32011","32","NV","011","Eureka","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,88.78924915839356,"A","CEC Survey",2017,15,"I",16.043865508414125,"TON",8,{"v":0.1806960376452,"d":"0.18"},{"$f":"VLOOKUP(A26291,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.175842777,"d":"0.18"}]
["32013","32","NV","013","Humboldt","","2104009000","Wax Log; Total: All Combustor Types",null,118.5605736289499,"A","CEC Survey",2017,15,"I",92.53586377818306,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A26308,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["32019","32","NV","019","Lyon","","2104008620","Hydronic heater: indoor","Hydronic heater",64.66715666345837,"A","CEC Survey",2017,15,"I",105.61790739196823,"TON",8,{"v":1.6332542335458828,"d":"1.63"},{"$f":"VLOOKUP(A26345,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.5893871482540705,"d":"1.59"}]
["32019","32","NV","019","Lyon","","2104008100","Fireplace: general","Fireplace: general",1664.752897467,"A","CEC Survey",2017,15,"I",426.58572595286404,"TON",8,{"v":0.25624567261720005,"d":"0.26"},{"$f":"VLOOKUP(A26347,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24936324700000004,"d":"0.25"}]
["32027","32","NV","027","Pershing","","2104008620","Hydronic heater: indoor","Hydronic heater",9.11435720822902,"A","CEC Survey",2017,15,"I",15.894459457779366,"TON",8,{"v":1.7438925307238167,"d":"1.74"},{"$f":"VLOOKUP(A26390,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6970538446125112,"d":"1.70"}]
["32027","32","NV","027","Pershing","","2104009000","Wax Log; Total: All Combustor Types",null,38.21358210880385,"A","CEC Survey",2017,15,"I",29.82548683986159,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A26398,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["32031","32","NV","031","Washoe","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1459.9674884592002,"A","CEC Survey",2017,15,"I",357.69940616982257,"TON",8,{"v":0.24500504908319998,"d":"0.25"},{"$f":"VLOOKUP(A26425,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.23842453199999997,"d":"0.24"}]
["32033","32","NV","033","White Pine","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",168.45050535992002,"A","CEC Survey",2017,15,"I",149.41461466629048,"TON",8,{"v":0.8869941609676001,"d":"0.89"},{"$f":"VLOOKUP(A26446,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.863170651,"d":"0.86"}]
["33001","33","NH","001","Belknap","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",781.13142296208,"A","CEC Survey",2017,15,"I",1829.3491215813672,"TON",8,{"v":2.3419223293365996,"d":"2.34"},{"$f":"VLOOKUP(A26474,cordwood_density!A:D,4,FALSE)","v":1.2206},{"v":1.9186648609999999,"d":"1.92"}]
["33003","33","NH","003","Carroll","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",747.638813376,"A","CEC Survey",2017,15,"I",1110.5654654923442,"TON",8,{"v":1.4854304586964004,"d":"1.49"},{"$f":"VLOOKUP(A26485,cordwood_density!A:D,4,FALSE)","v":1.3142},{"v":1.1302925420000003,"d":"1.13"}]
["33009","33","NH","009","Grafton","","2104008610","Hydronic heater: outdoor","Hydronic heater",1067.656891920666,"A","CEC Survey",2017,15,"I",5331.388787543439,"TON",8,{"v":4.993541303285659,"d":"4.99"},{"$f":"VLOOKUP(A26524,cordwood_density!A:D,4,FALSE)","v":1.2363},{"v":4.039101596122025,"d":"4.04"}]
["33009","33","NH","009","Grafton","","2104008100","Fireplace: general","Fireplace: general",3663.0677206240002,"A","CEC Survey",2017,15,"I",1864.6130034506168,"TON",8,{"v":0.5090304481548,"d":"0.51"},{"$f":"VLOOKUP(A26527,cordwood_density!A:D,4,FALSE)","v":1.2363},{"v":0.411736996,"d":"0.41"}]
["33013","33","NH","013","Merrimack","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$f":"P26563/J26563","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A26563,cordwood_density!A:D,4,FALSE)","v":1.2001},{"$f":"S26563/T26563","v":{"$error":"#DIV/0!"}}]
["33015","33","NH","015","Rockingham","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",8466.6563128125,"A","CEC Survey",2017,15,"I",16362.128566244139,"TON",8,{"v":1.9325372333211996,"d":"1.93"},{"$f":"VLOOKUP(A26580,cordwood_density!A:D,4,FALSE)","v":1.2164},{"v":1.5887349829999997,"d":"1.59"}]
["33019","33","NH","019","Sullivan","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",378.99727099719723,"A","CEC Survey",2017,15,"I",1681.4021661309957,"TON",8,{"v":4.436449269692578,"d":"4.44"},{"$f":"VLOOKUP(A26597,cordwood_density!A:D,4,FALSE)","v":1.2215},{"v":3.6319682928306003,"d":"3.63"}]
["34003","34","NJ","003","Bergen","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2.6620137200000005,"A","CEC Survey",2017,15,"I",0.8666155919126559,"TON",8,{"v":0.3255488825627299,"d":"0.33"},{"$f":"VLOOKUP(A26636,cordwood_density!A:D,4,FALSE)","v":1.1964},{"v":0.2721070566388582,"d":"0.27"}]
["34007","34","NJ","007","Camden","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",40.90461912212987,"A","CEC Survey",2017,15,"I",4.562812521067057,"TON",8,{"v":0.11154761048975328,"d":"0.11"},{"$f":"VLOOKUP(A26658,cordwood_density!A:D,4,FALSE)","v":1.448},{"v":0.07703564260342077,"d":"0.08"}]
["34009","34","NJ","009","Cape May","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",603.2348689905,"A","CEC Survey",2017,15,"I",419.6260601499058,"TON",8,{"v":0.6956263334911998,"d":"0.70"},{"$f":"VLOOKUP(A26679,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.5421028159999999,"d":"0.54"}]
["34011","34","NJ","011","Cumberland","","2104008610","Hydronic heater: outdoor","Hydronic heater",180.47207325514802,"A","CEC Survey",2017,15,"I",580.6832693244836,"TON",8,{"v":3.217579644599774,"d":"3.22"},{"$f":"VLOOKUP(A26689,cordwood_density!A:D,4,FALSE)","v":1.2976},{"v":2.4796390602649305,"d":"2.48"}]
["34013","34","NJ","013","Essex","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1048.05039177776,"A","CEC Survey",2017,15,"I",695.1848734021119,"TON",8,{"v":0.6633124502943999,"d":"0.66"},{"$f":"VLOOKUP(A26714,cordwood_density!A:D,4,FALSE)","v":1.2934},{"v":0.5128440159999998,"d":"0.51"}]
["34017","34","NJ","017","Hudson","","2104008620","Hydronic heater: indoor","Hydronic heater",878.8646583314825,"A","CEC Survey",2017,15,"I",0,"TON",8,{"v":0,"d":"0.00"},{"$f":"VLOOKUP(A26735,cordwood_density!A:D,4,FALSE)","v":1.2934},{"v":0,"d":"0.00"}]
["34021","34","NJ","021","Mercer","","2104008620","Hydronic heater: indoor","Hydronic heater",191.72436327586686,"A","CEC Survey",2017,15,"I",208.72814636740696,"TON",8,{"v":1.0886886924593606,"d":"1.09"},{"$f":"VLOOKUP(A26765,cordwood_density!A:D,4,FALSE)","v":1.3445},{"v":0.8097349888132098,"d":"0.81"}]
["34025","34","NJ","025","Monmouth","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",589.0532416431763,"A","CEC Survey",2017,15,"I",997.2067860834735,"TON",8,{"v":1.6928975440348046,"d":"1.69"},{"$f":"VLOOKUP(A26792,cordwood_density!A:D,4,FALSE)","v":1.3465},{"v":1.2572577378646896,"d":"1.26"}]
["34027","34","NJ","027","Morris","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1308.73031872128,"A","CEC Survey",2017,15,"I",1526.0827539463355,"TON",8,{"v":1.1660788568247,"d":"1.17"},{"$f":"VLOOKUP(A26813,cordwood_density!A:D,4,FALSE)","v":1.2817},{"v":0.9097907909999999,"d":"0.91"}]
["34027","34","NJ","027","Morris","","2104009000","Wax Log; Total: All Combustor Types",null,3553.8964981754057,"A","CEC Survey",2017,15,"I",2773.796315005514,"TON",8,{"v":0.7804943999999998,"d":"0.78"},{"$f":"VLOOKUP(A26818,cordwood_density!A:D,4,FALSE)","v":1.2817},{"v":0.6089524849808846,"d":"0.61"}]
["34033","34","NJ","033","Salem","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",120.7864074354878,"A","CEC Survey",2017,15,"I",410.5221191517405,"TON",8,{"v":3.398744344399853,"d":"3.40"},{"$f":"VLOOKUP(A26852,cordwood_density!A:D,4,FALSE)","v":1.3075},{"v":2.599422060726465,"d":"2.60"}]
["34035","34","NJ","035","Somerset","","2104008610","Hydronic heater: outdoor","Hydronic heater",400.5317851068811,"A","CEC Survey",2017,15,"I",966.832698146563,"TON",8,{"v":2.413872591631063,"d":"2.41"},{"$f":"VLOOKUP(A26869,cordwood_density!A:D,4,FALSE)","v":1.2066},{"v":2.0005574271764157,"d":"2.00"}]
["34037","34","NJ","037","Sussex","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1266.6374022687999,"A","CEC Survey",2017,15,"I",2521.456997417817,"TON",8,{"v":1.990669936717,"d":"1.99"},{"$f":"VLOOKUP(A26894,cordwood_density!A:D,4,FALSE)","v":1.3751},{"v":1.44765467,"d":"1.45"}]
["34039","34","NJ","039","Union","","2104009000","Wax Log; Total: All Combustor Types",null,3707.6348201857027,"A","CEC Survey",2017,15,"I",519.0688748259985,"TON",8,{"v":0.14000000000000004,"d":"0.14"},{"$f":"VLOOKUP(A26908,cordwood_density!A:D,4,FALSE)","v":1.2934},{"v":0.10824184320395858,"d":"0.11"}]
["35003","35","NM","003","Catron","","2104008100","Fireplace: general","Fireplace: general",61.887863759000005,"A","CEC Survey",2017,15,"I",63.39720869177355,"TON",8,{"$f":"P26947/J26947","v":{"v":1.0243883831351999,"d":"1.02"}},{"$f":"VLOOKUP(A26947,cordwood_density!A:D,4,FALSE)","v":1.0383},{"$f":"S26947/T26947","v":{"v":0.9866015439999999,"d":"0.99"}}]
["35005","35","NM","005","Chaves","","2104008610","Hydronic heater: outdoor","Hydronic heater",52.07020470873174,"A","CEC Survey",2017,15,"I",262.6546151792488,"TON",8,{"v":5.044240110990073,"d":"5.04"},{"$f":"VLOOKUP(A26959,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":4.959921446401252,"d":"4.96"}]
["35006","35","NM","006","Cibola","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",242.09760872528005,"A","CEC Survey",2017,15,"I",735.8287410511386,"TON",8,{"v":3.039388719804,"d":"3.04"},{"$f":"VLOOKUP(A26986,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.9885828120000006,"d":"2.99"}]
["35009","35","NM","009","Curry","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.765114386561132,"A","CEC Survey",2017,15,"I",20.029828535272898,"TON",8,{"v":5.319845953888042,"d":"5.32"},{"$f":"VLOOKUP(A27003,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.176961807987585,"d":"5.18"}]
["35011","35","NM","011","De Baca","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",13.770322411412385,"A","CEC Survey",2017,15,"I",11.337127010509088,"TON",8,{"v":0.8233014937336002,"d":"0.82"},{"$f":"VLOOKUP(A27024,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8011886860000001,"d":"0.80"}]
["35015","35","NM","015","Eddy","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2709.876357741,"A","CEC Survey",2017,15,"I",1700.7477817441109,"TON",8,{"v":0.6276108416849999,"d":"0.63"},{"$f":"VLOOKUP(A27056,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.617119805,"d":"0.62"}]
["35019","35","NM","019","Guadalupe","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.11049159709167893,"A","CEC Survey",2017,15,"I",0.60399989349219,"TON",8,{"v":5.466478079695319,"d":"5.47"},{"$f":"VLOOKUP(A27081,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":5.319655585534565,"d":"5.32"}]
["35021","35","NM","021","Harding","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",9.558785642,"A","CEC Survey",2017,15,"I",8.292370043945494,"TON",8,{"v":0.8675129199999999,"d":"0.87"},{"$f":"VLOOKUP(A27102,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8442126508369013,"d":"0.84"}]
["35023","35","NM","023","Hidalgo","","2104008610","Hydronic heater: outdoor","Hydronic heater",6.018361082713381,"A","CEC Survey",2017,15,"I",32.42510327830203,"TON",8,{"v":5.387696556033684,"d":"5.39"},{"$f":"VLOOKUP(A27109,cordwood_density!A:D,4,FALSE)","v":1.0557},{"v":5.103435214581494,"d":"5.10"}]
["35027","35","NM","027","Lincoln","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.951704151443805,"A","CEC Survey",2017,15,"I",5.18355927309167,"TON",8,{"v":5.446607819486581,"d":"5.45"},{"$f":"VLOOKUP(A27141,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":5.355563244332922,"d":"5.36"}]
["35028","35","NM","028","Los Alamos","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",74.67108722675,"A","CEC Survey",2017,15,"I",89.16416161449744,"TON",8,{"v":1.1940921838158998,"d":"1.19"},{"$f":"VLOOKUP(A27158,cordwood_density!A:D,4,FALSE)","v":1.0187},{"v":1.172172557,"d":"1.17"}]
["35031","35","NM","031","Mckinley","","2104008620","Hydronic heater: indoor","Hydronic heater",77.06993044693672,"A","CEC Survey",2017,15,"I",448.9986783901955,"TON",8,{"v":5.825860692833176,"d":"5.83"},{"$f":"VLOOKUP(A27185,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":5.728476590789751,"d":"5.73"}]
["35033","35","NM","033","Mora","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",20.907479925319937,"A","CEC Survey",2017,15,"I",131.05682026974466,"TON",8,{"v":6.268417845568692,"d":"6.27"},{"$f":"VLOOKUP(A27197,cordwood_density!A:D,4,FALSE)","v":1.0173},{"v":6.161818387465537,"d":"6.16"}]
["35037","35","NM","037","Quay","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,409.20385244,"A","CEC Survey",2017,15,"I",259.03518359335413,"TON",8,{"v":0.6330223482716001,"d":"0.63"},{"$f":"VLOOKUP(A27236,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.616020191,"d":"0.62"}]
["35039","35","NM","039","Rio Arriba","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",169.89843183264003,"A","CEC Survey",2017,15,"I",160.9751962782346,"TON",8,{"v":0.9474789999051001,"d":"0.95"},{"$f":"VLOOKUP(A27250,cordwood_density!A:D,4,FALSE)","v":1.0179},{"v":0.9308173690000001,"d":"0.93"}]
["35043","35","NM","043","Sandoval","","2104008620","Hydronic heater: indoor","Hydronic heater",146.7783211116664,"A","CEC Survey",2017,15,"I",827.6532721224031,"TON",8,{"v":5.638797786035029,"d":"5.64"},{"$f":"VLOOKUP(A27275,cordwood_density!A:D,4,FALSE)","v":1.0186},{"v":5.535831323419428,"d":"5.54"}]
["35045","35","NM","045","San Juan","","2104008100","Fireplace: general","Fireplace: general",2561.803511226,"A","CEC Survey",2017,15,"I",2248.675321043339,"TON",8,{"v":0.8777704110364001,"d":"0.88"},{"$f":"VLOOKUP(A27292,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.854194639,"d":"0.85"}]
["35049","35","NM","049","Santa Fe","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,7492.539492916,"A","CEC Survey",2017,15,"I",4623.954649812265,"TON",8,{"v":0.6171411781258002,"d":"0.62"},{"$f":"VLOOKUP(A27326,cordwood_density!A:D,4,FALSE)","v":1.0091},{"v":0.611575838,"d":"0.61"}]
["35049","35","NM","049","Santa Fe","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1326.4504086607203,"A","CEC Survey",2017,15,"I",3612.956309750375,"TON",8,{"$f":"P27331/J27331","v":{"v":2.7237779009004006,"d":"2.72"}},{"$f":"VLOOKUP(A27331,cordwood_density!A:D,4,FALSE)","v":1.0091},{"$f":"S27331/T27331","v":{"v":2.6992150440000002,"d":"2.70"}}]
["35055","35","NM","055","Taos","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",191.72387452344003,"A","CEC Survey",2017,15,"I",209.60781735931636,"TON",8,{"v":1.0932796861128,"d":"1.09"},{"$f":"VLOOKUP(A27370,cordwood_density!A:D,4,FALSE)","v":1.0198},{"v":1.072053036,"d":"1.07"}]
["35057","35","NM","057","Torrance","","2104008610","Hydronic heater: outdoor","Hydronic heater",33.34068881591517,"A","CEC Survey",2017,15,"I",189.53078456438945,"TON",8,{"v":5.68466913238808,"d":"5.68"},{"$f":"VLOOKUP(A27379,cordwood_density!A:D,4,FALSE)","v":1.0174},{"v":5.587447545103282,"d":"5.59"}]
["35061","35","NM","061","Valencia","","2104008610","Hydronic heater: outdoor","Hydronic heater",51.53416505144178,"A","CEC Survey",2017,15,"I",262.2163623321164,"TON",8,{"v":5.088204341146695,"d":"5.09"},{"$f":"VLOOKUP(A27409,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":5.003150777922021,"d":"5.00"}]
["36001","36","NY","001","Albany","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1455.0401900774402,"A","CEC Survey",2017,15,"I",843.1517482992036,"TON",8,{"v":0.5794697315228999,"d":"0.58"},{"$f":"VLOOKUP(A27430,cordwood_density!A:D,4,FALSE)","v":1.3659},{"v":0.42424023099999997,"d":"0.42"}]
["36003","36","NY","003","Allegany","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",741.242982204,"A","CEC Survey",2017,15,"I",482.7966112872356,"TON",8,{"v":0.651333804,"d":"0.65"},{"$f":"VLOOKUP(A27447,cordwood_density!A:D,4,FALSE)","v":1.3822},{"v":0.4712297815077412,"d":"0.47"}]
["36007","36","NY","007","Broome","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,9564.515012676,"A","CEC Survey",2017,15,"I",1843.3671122758244,"TON",8,{"v":0.1927298048916,"d":"0.19"},{"$f":"VLOOKUP(A27476,cordwood_density!A:D,4,FALSE)","v":1.3164},{"v":0.146406719,"d":"0.15"}]
["36009","36","NY","009","Cattaraugus","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",12.371204745054275,"A","CEC Survey",2017,15,"I",25.206003284528535,"TON",8,{"v":2.0374736174829957,"d":"2.04"},{"$f":"VLOOKUP(A27486,cordwood_density!A:D,4,FALSE)","v":1.3823},{"v":1.473973535037977,"d":"1.47"}]
["36013","36","NY","013","Chautauqua","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2701.434631077,"A","CEC Survey",2017,15,"I",2882.2027167860706,"TON",8,{"v":1.0669155876027998,"d":"1.07"},{"$f":"VLOOKUP(A27525,cordwood_density!A:D,4,FALSE)","v":1.3823},{"v":0.7718408359999999,"d":"0.77"}]
["36015","36","NY","015","Chemung","","2104008610","Hydronic heater: outdoor","Hydronic heater",294.854311799986,"A","CEC Survey",2017,15,"I",527.628300994487,"TON",8,{"v":1.7894542486880871,"d":"1.79"},{"$f":"VLOOKUP(A27529,cordwood_density!A:D,4,FALSE)","v":1.3165},{"v":1.3592512333369442,"d":"1.36"}]
["36019","36","NY","019","Clinton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1241.62538544,"A","CEC Survey",2017,15,"I",650.879878045544,"TON",8,{"v":0.5242159879124,"d":"0.52"},{"$f":"VLOOKUP(A27564,cordwood_density!A:D,4,FALSE)","v":1.3004},{"v":0.40311903099999996,"d":"0.40"}]
["36021","36","NY","021","Columbia","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3933.7428546899996,"A","CEC Survey",2017,15,"I",797.7737775170073,"TON",8,{"v":0.2028027268142,"d":"0.20"},{"$f":"VLOOKUP(A27581,cordwood_density!A:D,4,FALSE)","v":1.3646},{"v":0.148616977,"d":"0.15"}]
["36027","36","NY","027","Dutchess","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",916.546113774622,"A","CEC Survey",2017,15,"I",1769.8426781104351,"TON",8,{"v":1.9309914160474397,"d":"1.93"},{"$f":"VLOOKUP(A27617,cordwood_density!A:D,4,FALSE)","v":1.3582},{"v":1.4217283287052271,"d":"1.42"}]
["36027","36","NY","027","Dutchess","","2104008620","Hydronic heater: indoor","Hydronic heater",569.7448815355758,"A","CEC Survey",2017,15,"I",1100.1724755821624,"TON",8,{"v":1.93099141604744,"d":"1.93"},{"$f":"VLOOKUP(A27620,cordwood_density!A:D,4,FALSE)","v":1.3582},{"v":1.4217283287052274,"d":"1.42"}]
["36031","36","NY","031","Essex","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",639.63771957184,"A","CEC Survey",2017,15,"I",816.1329274178937,"TON",8,{"v":1.2759299560447996,"d":"1.28"},{"$f":"VLOOKUP(A27659,cordwood_density!A:D,4,FALSE)","v":1.3456},{"v":0.9482238079999998,"d":"0.95"}]
["36033","36","NY","033","Franklin","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",617.85890274192,"A","CEC Survey",2017,15,"I",354.0360549555677,"TON",8,{"v":0.5730046995915,"d":"0.57"},{"$f":"VLOOKUP(A27670,cordwood_density!A:D,4,FALSE)","v":1.3005},{"v":0.440603383,"d":"0.44"}]
["36037","36","NY","037","Genesee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",185.41312941632,"A","CEC Survey",2017,15,"I",71.27160121764113,"TON",8,{"v":0.3843934970625,"d":"0.38"},{"$f":"VLOOKUP(A27698,cordwood_density!A:D,4,FALSE)","v":1.2825},{"v":0.299722025,"d":"0.30"}]
["36039","36","NY","039","Greene","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",620.7415262726399,"A","CEC Survey",2017,15,"I",765.8912156610592,"TON",8,{"v":1.2338327359215002,"d":"1.23"},{"$f":"VLOOKUP(A27719,cordwood_density!A:D,4,FALSE)","v":1.3585},{"v":0.9082316790000001,"d":"0.91"}]
["36043","36","NY","043","Herkimer","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3664.784010626,"A","CEC Survey",2017,15,"I",703.7459675254996,"TON",8,{"v":0.19202931618480001,"d":"0.19"},{"$f":"VLOOKUP(A27746,cordwood_density!A:D,4,FALSE)","v":1.3054},{"v":0.14710381200000003,"d":"0.15"}]
["36045","36","NY","045","Jefferson","","2104008610","Hydronic heater: outdoor","Hydronic heater",363.04560935410433,"A","CEC Survey",2017,15,"I",688.5819440015817,"TON",8,{"v":1.8966816462169593,"d":"1.90"},{"$f":"VLOOKUP(A27754,cordwood_density!A:D,4,FALSE)","v":1.3004},{"v":1.4585371010588737,"d":"1.46"}]
["36047","36","NY","047","Kings","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",199.286065699,"A","CEC Survey",2017,15,"I",57.70619879117134,"TON",8,{"v":0.28956464461660003,"d":"0.29"},{"$f":"VLOOKUP(A27775,cordwood_density!A:D,4,FALSE)","v":1.2934},{"v":0.223878649,"d":"0.22"}]
["36051","36","NY","051","Livingston","","2104008610","Hydronic heater: outdoor","Hydronic heater",261.92504429521983,"A","CEC Survey",2017,15,"I",485.6436008860194,"TON",8,{"v":1.8541319796004037,"d":"1.85"},{"$f":"VLOOKUP(A27799,cordwood_density!A:D,4,FALSE)","v":1.2822},{"v":1.4460552016849193,"d":"1.45"}]
["36055","36","NY","055","Monroe","","2104008100","Fireplace: general","Fireplace: general",38786.544037696,"A","CEC Survey",2017,15,"I",6220.096226563258,"TON",8,{"v":0.16036737432749998,"d":"0.16"},{"$f":"VLOOKUP(A27832,cordwood_density!A:D,4,FALSE)","v":1.2825},{"v":0.125042787,"d":"0.13"}]
["36057","36","NY","057","Montgomery","","2104009000","Wax Log; Total: All Combustor Types",null,107.02201045857454,"A","CEC Survey",2017,15,"I",83.53007983965885,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A27853,cordwood_density!A:D,4,FALSE)","v":1.3655},{"v":0.5715813987550348,"d":"0.57"}]
["36059","36","NY","059","Nassau","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",11753.713924259999,"A","CEC Survey",2017,15,"I",4556.556211338673,"TON",8,{"v":0.38766948393510003,"d":"0.39"},{"$f":"VLOOKUP(A27870,cordwood_density!A:D,4,FALSE)","v":1.3719},{"v":0.282578529,"d":"0.28"}]
["36065","36","NY","065","Oneida","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",659.48562694016,"A","CEC Survey",2017,15,"I",313.6538671624618,"TON",8,{"v":0.47560379536659997,"d":"0.48"},{"$f":"VLOOKUP(A27908,cordwood_density!A:D,4,FALSE)","v":1.3054},{"v":0.364335679,"d":"0.36"}]
["36065","36","NY","065","Oneida","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2060.892584188,"A","CEC Survey",2017,15,"I",980.1683348826931,"TON",8,{"v":0.4756037953666,"d":"0.48"},{"$f":"VLOOKUP(A27909,cordwood_density!A:D,4,FALSE)","v":1.3054},{"v":0.364335679,"d":"0.36"}]
["36071","36","NY","071","Orange","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",74.76348526487833,"A","CEC Survey",2017,15,"I",138.9359659230262,"TON",8,{"v":1.8583398758202918,"d":"1.86"},{"$f":"VLOOKUP(A27948,cordwood_density!A:D,4,FALSE)","v":1.3589},{"v":1.3675324717199882,"d":"1.37"}]
["36071","36","NY","071","Orange","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",3979.9102993092,"A","CEC Survey",2017,15,"I",3676.2033494237994,"TON",8,{"v":0.9236900012701,"d":"0.92"},{"$f":"VLOOKUP(A27961,cordwood_density!A:D,4,FALSE)","v":1.3589},{"v":0.679733609,"d":"0.68"}]
["36075","36","NY","075","Oswego","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1570.7645729820001,"A","CEC Survey",2017,15,"I",882.0102693262553,"TON",8,{"v":0.561516528,"d":"0.56"},{"$f":"VLOOKUP(A27987,cordwood_density!A:D,4,FALSE)","v":1.2821},{"v":0.4379662491225333,"d":"0.44"}]
["36077","36","NY","077","Otsego","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",734.83717053184,"A","CEC Survey",2017,15,"I",848.2150765535988,"TON",8,{"v":1.154289835311,"d":"1.15"},{"$f":"VLOOKUP(A28004,cordwood_density!A:D,4,FALSE)","v":1.3162},{"v":0.8769866550000001,"d":"0.88"}]
["36083","36","NY","083","Rensselaer","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",491.11656661698237,"A","CEC Survey",2017,15,"I",881.0374421106476,"TON",8,{"v":1.793947714245529,"d":"1.79"},{"$f":"VLOOKUP(A28037,cordwood_density!A:D,4,FALSE)","v":1.3646},{"v":1.3146326500406924,"d":"1.31"}]
["36083","36","NY","083","Rensselaer","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",489.08404263936,"A","CEC Survey",2017,15,"I",282.09056853219596,"TON",8,{"v":0.5767732003888,"d":"0.58"},{"$f":"VLOOKUP(A28043,cordwood_density!A:D,4,FALSE)","v":1.3646},{"v":0.422668328,"d":"0.42"}]
["36089","36","NY","089","St Lawrence","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",22.220658277789667,"A","CEC Survey",2017,15,"I",45.92593722498115,"TON",8,{"v":2.0668126322290705,"d":"2.07"},{"$f":"VLOOKUP(A28086,cordwood_density!A:D,4,FALSE)","v":1.3004},{"v":1.5893668349962093,"d":"1.59"}]
["36089","36","NY","089","St Lawrence","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",971.1239259134801,"A","CEC Survey",2017,15,"I",481.64921579362647,"TON",8,{"v":0.49597090849200004,"d":"0.50"},{"$f":"VLOOKUP(A28090,cordwood_density!A:D,4,FALSE)","v":1.3004},{"v":0.38139873,"d":"0.38"}]
["36093","36","NY","093","Schenectady","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5816.60002445,"A","CEC Survey",2017,15,"I",1215.8142651412913,"TON",8,{"v":0.2090249045887,"d":"0.21"},{"$f":"VLOOKUP(A28121,cordwood_density!A:D,4,FALSE)","v":1.3679},{"v":0.152807153,"d":"0.15"}]
["36097","36","NY","097","Schuyler","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",128.71684157839934,"A","CEC Survey",2017,15,"I",261.30459080864284,"TON",8,{"v":2.030073047197064,"d":"2.03"},{"$f":"VLOOKUP(A28142,cordwood_density!A:D,4,FALSE)","v":1.3156},{"v":1.5430777190613132,"d":"1.54"}]
["36099","36","NY","099","Seneca","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1847.5561722240002,"A","CEC Survey",2017,15,"I",353.56288599451824,"TON",8,{"v":0.19136786816549997,"d":"0.19"},{"$f":"VLOOKUP(A28166,cordwood_density!A:D,4,FALSE)","v":1.2823},{"v":0.149237985,"d":"0.15"}]
["36101","36","NY","101","Steuben","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5702.275366979,"A","CEC Survey",2017,15,"I",1167.5787866765477,"TON",8,{"v":0.2047566473969,"d":"0.20"},{"$f":"VLOOKUP(A28181,cordwood_density!A:D,4,FALSE)","v":1.3823},{"v":0.148127503,"d":"0.15"}]
["36107","36","NY","107","Tioga","","2104008620","Hydronic heater: indoor","Hydronic heater",209.70799937210631,"A","CEC Survey",2017,15,"I",421.2494450588779,"TON",8,{"v":2.00874285349226,"d":"2.01"},{"$f":"VLOOKUP(A28220,cordwood_density!A:D,4,FALSE)","v":1.3164},{"v":1.525936534102294,"d":"1.53"}]
["36109","36","NY","109","Tompkins","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",948.531563216,"A","CEC Survey",2017,15,"I",505.13834979466355,"TON",8,{"v":0.53254775,"d":"0.53"},{"$f":"VLOOKUP(A28242,cordwood_density!A:D,4,FALSE)","v":1.3164},{"v":0.404548579459131,"d":"0.40"}]
["36111","36","NY","111","Ulster","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1942.9399883655703,"A","CEC Survey",2017,15,"I",2227.6527225257987,"TON",8,{"v":1.1465370705555002,"d":"1.15"},{"$f":"VLOOKUP(A28259,cordwood_density!A:D,4,FALSE)","v":1.3583},{"v":0.8440970850000001,"d":"0.84"}]
["36113","36","NY","113","Warren","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1417.0110972394202,"A","CEC Survey",2017,15,"I",1617.4827197781785,"TON",8,{"v":1.1414749841615999,"d":"1.14"},{"$f":"VLOOKUP(A28276,cordwood_density!A:D,4,FALSE)","v":1.3456},{"v":0.8483018609999999,"d":"0.85"}]
["36117","36","NY","117","Wayne","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",35.05258852203625,"A","CEC Survey",2017,15,"I",64.27838909682409,"TON",8,{"v":1.8337701096286987,"d":"1.83"},{"$f":"VLOOKUP(A28293,cordwood_density!A:D,4,FALSE)","v":1.2817},{"v":1.4307327062719033,"d":"1.43"}]
["36121","36","NY","121","Wyoming","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",144.82719912672,"A","CEC Survey",2017,15,"I",60.000326279642266,"TON",8,{"v":0.41428907443790003,"d":"0.41"},{"$f":"VLOOKUP(A28328,cordwood_density!A:D,4,FALSE)","v":1.2821},{"v":0.32313319900000004,"d":"0.32"}]
["37001","37","NC","001","Alamance","","2104008610","Hydronic heater: outdoor","Hydronic heater",240.43282466198423,"A","CEC Survey",2017,15,"I",433.0723551488095,"TON",8,{"v":1.8012197617261712,"d":"1.80"},{"$f":"VLOOKUP(A28354,cordwood_density!A:D,4,FALSE)","v":1.2195},{"v":1.477014974765208,"d":"1.48"}]
["37003","37","NC","003","Alexander","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",386.15447901632007,"A","CEC Survey",2017,15,"I",223.6059354144812,"TON",8,{"v":0.5790582462855,"d":"0.58"},{"$f":"VLOOKUP(A28375,cordwood_density!A:D,4,FALSE)","v":1.2559},{"v":0.46107034499999994,"d":"0.46"}]
["37003","37","NC","003","Alexander","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",588.0923502540801,"A","CEC Survey",2017,15,"I",685.9761692977021,"TON",8,{"v":1.1664429387686002,"d":"1.17"},{"$f":"VLOOKUP(A28381,cordwood_density!A:D,4,FALSE)","v":1.2559},{"v":0.9287705540000001,"d":"0.93"}]
["37007","37","NC","007","Anson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",579.6378453589899,"A","CEC Survey",2017,15,"I",704.5336617470008,"TON",8,{"v":1.2154721562576,"d":"1.22"},{"$f":"VLOOKUP(A28410,cordwood_density!A:D,4,FALSE)","v":1.2996},{"v":0.935266356,"d":"0.94"}]
["37011","37","NC","011","Avery","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.210669575708162,"A","CEC Survey",2017,15,"I",4.5748021969783546,"TON",8,{"v":2.0694192597791874,"d":"2.07"},{"$f":"VLOOKUP(A28431,cordwood_density!A:D,4,FALSE)","v":1.1996},{"v":1.7250910801760482,"d":"1.73"}]
["37015","37","NC","015","Bertie","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",52.8511728925541,"A","CEC Survey",2017,15,"I",102.5492936059833,"TON",8,{"v":1.9403409232651274,"d":"1.94"},{"$f":"VLOOKUP(A28457,cordwood_density!A:D,4,FALSE)","v":1.1973},{"v":1.6205971128916123,"d":"1.62"}]
["37015","37","NC","015","Bertie","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",513.2634634272,"A","CEC Survey",2017,15,"I",592.8185409174062,"TON",8,{"v":1.1549985205629,"d":"1.15"},{"$f":"VLOOKUP(A28470,cordwood_density!A:D,4,FALSE)","v":1.1973},{"v":0.964669273,"d":"0.96"}]
["37021","37","NC","021","Buncombe","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3501.51313553735,"A","CEC Survey",2017,15,"I",2540.3113084314837,"TON",8,{"v":0.7254895841028001,"d":"0.73"},{"$f":"VLOOKUP(A28509,cordwood_density!A:D,4,FALSE)","v":1.2342},{"v":0.587821734,"d":"0.59"}]
["37025","37","NC","025","Cabarrus","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",18.692820082829805,"A","CEC Survey",2017,15,"I",33.47086468969357,"TON",8,{"v":1.7905733079000778,"d":"1.79"},{"$f":"VLOOKUP(A28533,cordwood_density!A:D,4,FALSE)","v":1.289},{"v":1.38911815973629,"d":"1.39"}]
["37027","37","NC","027","Caldwell","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",18.61569868696999,"A","CEC Survey",2017,15,"I",40.211177559171546,"TON",8,{"v":2.1600681357889218,"d":"2.16"},{"$f":"VLOOKUP(A28548,cordwood_density!A:D,4,FALSE)","v":1.2951},{"v":1.6678774888340067,"d":"1.67"}]
["37029","37","NC","029","Camden","","2104008620","Hydronic heater: indoor","Hydronic heater",17.359212602020307,"A","CEC Survey",2017,15,"I",31.180057948557515,"TON",8,{"v":1.7961677561877838,"d":"1.80"},{"$f":"VLOOKUP(A28565,cordwood_density!A:D,4,FALSE)","v":1.1375},{"v":1.5790485768683815,"d":"1.58"}]
["37031","37","NC","031","Carteret","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3476.14461,"A","CEC Survey",2017,15,"I",692.0506786782195,"TON",8,{"v":0.19908569876159998,"d":"0.20"},{"$f":"VLOOKUP(A28586,cordwood_density!A:D,4,FALSE)","v":1.1046},{"v":0.180233296,"d":"0.18"}]
["37033","37","NC","033","Caswell","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",508.5316032212,"A","CEC Survey",2017,15,"I",596.8763139532351,"TON",8,{"v":1.17372511398,"d":"1.17"},{"$f":"VLOOKUP(A28604,cordwood_density!A:D,4,FALSE)","v":1.1775},{"v":0.996794152,"d":"1.00"}]
["37039","37","NC","039","Cherokee","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",434.3108146998401,"A","CEC Survey",2017,15,"I",410.2667503787625,"TON",8,{"v":0.9446385779325001,"d":"0.94"},{"$f":"VLOOKUP(A28643,cordwood_density!A:D,4,FALSE)","v":1.4025},{"v":0.673539093,"d":"0.67"}]
["37039","37","NC","039","Cherokee","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",672.74358675888,"A","CEC Survey",2017,15,"I",995.7743368686191,"TON",8,{"v":1.4801692003725,"d":"1.48"},{"$f":"VLOOKUP(A28651,cordwood_density!A:D,4,FALSE)","v":1.4025},{"v":1.055379109,"d":"1.06"}]
["37045","37","NC","045","Cleveland","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",187.14020138453282,"A","CEC Survey",2017,15,"I",378.0929697264514,"TON",8,{"v":2.0203727843038477,"d":"2.02"},{"$f":"VLOOKUP(A28682,cordwood_density!A:D,4,FALSE)","v":1.339},{"v":1.5088669038863687,"d":"1.51"}]
["37047","37","NC","047","Columbus","","2104008610","Hydronic heater: outdoor","Hydronic heater",121.70585331653079,"A","CEC Survey",2017,15,"I",240.26016691213704,"TON",8,{"v":1.974105274027141,"d":"1.97"},{"$f":"VLOOKUP(A28699,cordwood_density!A:D,4,FALSE)","v":1.2595},{"v":1.5673721905733553,"d":"1.57"}]
["37049","37","NC","049","Craven","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",942.9632250956402,"A","CEC Survey",2017,15,"I",549.5244472587119,"TON",8,{"v":0.5827633916507999,"d":"0.58"},{"$f":"VLOOKUP(A28720,cordwood_density!A:D,4,FALSE)","v":1.1899},{"v":0.489758292,"d":"0.49"}]
["37053","37","NC","053","Currituck","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",251.99500172478,"A","CEC Survey",2017,15,"I",86.65645751279972,"TON",8,{"v":0.343881652095,"d":"0.34"},{"$f":"VLOOKUP(A28748,cordwood_density!A:D,4,FALSE)","v":1.191},{"v":0.288733545,"d":"0.29"}]
["37057","37","NC","057","Davidson","","2104008100","Fireplace: general","Fireplace: general",6265.203037925,"A","CEC Survey",2017,15,"I",1647.1740915725711,"TON",8,{"v":0.2629083337925,"d":"0.26"},{"$f":"VLOOKUP(A28777,cordwood_density!A:D,4,FALSE)","v":1.1825},{"v":0.22233262899999998,"d":"0.22"}]
["37059","37","NC","059","Davie","","2104009000","Wax Log; Total: All Combustor Types",null,228.29944274790813,"A","CEC Survey",2017,15,"I",78.40459224861065,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A28798,cordwood_density!A:D,4,FALSE)","v":1.3412},{"v":0.2560608037578288,"d":"0.26"}]
["37059","37","NC","059","Davie","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",617.1811158128,"A","CEC Survey",2017,15,"I",729.214544033623,"TON",8,{"v":1.1815243942992002,"d":"1.18"},{"$f":"VLOOKUP(A28801,cordwood_density!A:D,4,FALSE)","v":1.3412},{"v":0.8809457160000002,"d":"0.88"}]
["37065","37","NC","065","Edgecombe","","2104008100","Fireplace: general","Fireplace: general",1734.90052835,"A","CEC Survey",2017,15,"I",509.00141345713047,"TON",8,{"v":0.293389393305,"d":"0.29"},{"$f":"VLOOKUP(A28837,cordwood_density!A:D,4,FALSE)","v":1.229},{"v":0.238722045,"d":"0.24"}]
["37067","37","NC","067","Forsyth","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3692.7365699960596,"A","CEC Survey",2017,15,"I",1822.1728941978079,"TON",8,{"v":0.49344784272,"d":"0.49"},{"$f":"VLOOKUP(A28854,cordwood_density!A:D,4,FALSE)","v":1.0425},{"v":0.473331264,"d":"0.47"}]
["37071","37","NC","071","Gaston","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",255.689442128343,"A","CEC Survey",2017,15,"I",422.80468749921585,"TON",8,{"v":1.6535868042881081,"d":"1.65"},{"$f":"VLOOKUP(A28877,cordwood_density!A:D,4,FALSE)","v":1.2001},{"v":1.3778741807250297,"d":"1.38"}]
["37073","37","NC","073","Gates","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.883988209224206,"A","CEC Survey",2017,15,"I",5.4109114876506,"TON",8,{"v":1.8761905719115743,"d":"1.88"},{"$f":"VLOOKUP(A28893,cordwood_density!A:D,4,FALSE)","v":1.164},{"v":1.6118475703707684,"d":"1.61"}]
["37077","37","NC","077","Granville","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",720.984854815,"A","CEC Survey",2017,15,"I",314.9774213718994,"TON",8,{"v":0.436871065,"d":"0.44"},{"$f":"VLOOKUP(A28932,cordwood_density!A:D,4,FALSE)","v":1.2137},{"v":0.3599497940182912,"d":"0.36"}]
["37079","37","NC","079","Greene","","2104008100","Fireplace: general","Fireplace: general",378.0193296514452,"A","CEC Survey",2017,15,"I",135.69490585794492,"TON",8,{"v":0.35896287627160006,"d":"0.36"},{"$f":"VLOOKUP(A28942,cordwood_density!A:D,4,FALSE)","v":1.2602},{"v":0.28484595800000007,"d":"0.28"}]
["37083","37","NC","083","Halifax","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.8553551565809396,"A","CEC Survey",2017,15,"I",5.436350592905095,"TON",8,{"v":1.9039139773472844,"d":"1.90"},{"$f":"VLOOKUP(A28971,cordwood_density!A:D,4,FALSE)","v":1.239},{"v":1.536653734743571,"d":"1.54"}]
["37085","37","NC","085","Harnett","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1230.41075684081,"A","CEC Survey",2017,15,"I",665.0288686823758,"TON",8,{"v":0.5404933799423999,"d":"0.54"},{"$f":"VLOOKUP(A28988,cordwood_density!A:D,4,FALSE)","v":1.2304},{"v":0.43928265599999994,"d":"0.44"}]
["37089","37","NC","089","Henderson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1250.80073224312,"A","CEC Survey",2017,15,"I",966.9057719356823,"TON",8,{"v":0.7730294258796,"d":"0.77"},{"$f":"VLOOKUP(A29018,cordwood_density!A:D,4,FALSE)","v":1.3164},{"v":0.587229889,"d":"0.59"}]
["37091","37","NC","091","Hertford","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",50.45021661412236,"A","CEC Survey",2017,15,"I",103.2184174809576,"TON",8,{"v":2.045945972253051,"d":"2.05"},{"$f":"VLOOKUP(A29027,cordwood_density!A:D,4,FALSE)","v":1.331},{"v":1.537149490798686,"d":"1.54"}]
["37095","37","NC","095","Hyde","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,284.63287247,"A","CEC Survey",2017,15,"I",56.72294592538061,"TON",8,{"v":0.19928459222979997,"d":"0.20"},{"$f":"VLOOKUP(A29066,cordwood_density!A:D,4,FALSE)","v":1.0997},{"v":0.18121723399999998,"d":"0.18"}]
["37095","37","NC","095","Hyde","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",76.1274092376,"A","CEC Survey",2017,15,"I",73.51098450179147,"TON",8,{"v":0.965630976254,"d":"0.97"},{"$f":"VLOOKUP(A29071,cordwood_density!A:D,4,FALSE)","v":1.0997},{"v":0.87808582,"d":"0.88"}]
["37101","37","NC","101","Johnston","","2104008620","Hydronic heater: indoor","Hydronic heater",182.68647695909348,"A","CEC Survey",2017,15,"I",342.0098424827503,"TON",8,{"v":1.8721136242576506,"d":"1.87"},{"$f":"VLOOKUP(A29105,cordwood_density!A:D,4,FALSE)","v":1.2424},{"v":1.5068525629890943,"d":"1.51"}]
["37103","37","NC","103","Jones","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,614.5791407758372,"A","CEC Survey",2017,15,"I",135.4253298746357,"TON",8,{"v":0.22035458233039998,"d":"0.22"},{"$f":"VLOOKUP(A29126,cordwood_density!A:D,4,FALSE)","v":1.2226},{"v":0.180234404,"d":"0.18"}]
["37105","37","NC","105","Lee","","2104009000","Wax Log; Total: All Combustor Types",null,311.5472294837921,"A","CEC Survey",2017,15,"I",106.99427558758187,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A29143,cordwood_density!A:D,4,FALSE)","v":1.2815},{"v":0.2679896605540382,"d":"0.27"}]
["37109","37","NC","109","Lincoln","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",821.2940825000001,"A","CEC Survey",2017,15,"I",454.2021225848776,"TON",8,{"v":0.5530322600186001,"d":"0.55"},{"$f":"VLOOKUP(A29168,cordwood_density!A:D,4,FALSE)","v":1.2899},{"v":0.428740414,"d":"0.43"}]
["37111","37","NC","111","McDowell","","2104008100","Fireplace: general","Fireplace: general",1888.53314208,"A","CEC Survey",2017,15,"I",569.2936277666432,"TON",8,{"v":0.301447517696,"d":"0.30"},{"$f":"VLOOKUP(A29182,cordwood_density!A:D,4,FALSE)","v":1.3312},{"v":0.226447955,"d":"0.23"}]
["37115","37","NC","115","Madison","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",466.30773965284806,"A","CEC Survey",2017,15,"I",487.7703593891272,"TON",8,{"v":1.0460267285125,"d":"1.05"},{"$f":"VLOOKUP(A29221,cordwood_density!A:D,4,FALSE)","v":0.9989},{"v":1.047178625,"d":"1.05"}]
["37119","37","NC","119","Mecklenburg","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",6876.510923053459,"A","CEC Survey",2017,15,"I",3731.221502642512,"TON",8,{"v":0.5426038792629,"d":"0.54"},{"$f":"VLOOKUP(A29244,cordwood_density!A:D,4,FALSE)","v":1.1763},{"v":0.461280183,"d":"0.46"}]
["37121","37","NC","121","Mitchell","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",211.13287667640003,"A","CEC Survey",2017,15,"I",164.07687088895858,"TON",8,{"v":0.777126108789,"d":"0.78"},{"$f":"VLOOKUP(A29260,cordwood_density!A:D,4,FALSE)","v":1.1373},{"v":0.68330793,"d":"0.68"}]
["37123","37","NC","123","Montgomery","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",416.980355285,"A","CEC Survey",2017,15,"I",189.0131803638298,"TON",8,{"v":0.453290372,"d":"0.45"},{"$f":"VLOOKUP(A29277,cordwood_density!A:D,4,FALSE)","v":1.2571},{"v":0.3605841794606634,"d":"0.36"}]
["37127","37","NC","127","Nash","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1180.48209385222,"A","CEC Survey",2017,15,"I",1143.9904611484062,"TON",8,{"v":0.9690875169612,"d":"0.97"},{"$f":"VLOOKUP(A29309,cordwood_density!A:D,4,FALSE)","v":1.1703},{"v":0.828067604,"d":"0.83"}]
["37129","37","NC","129","New Hanover","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.404805228142016,"A","CEC Survey",2017,15,"I",4.824440875729452,"TON",8,{"v":1.0952676964934591,"d":"1.10"},{"$f":"VLOOKUP(A29316,cordwood_density!A:D,4,FALSE)","v":1.346},{"v":0.8137204283012326,"d":"0.81"}]
["37133","37","NC","133","Onslow","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2440.4717894826754,"A","CEC Survey",2017,15,"I",2271.0172100474906,"TON",8,{"v":0.9305648276020001,"d":"0.93"},{"$f":"VLOOKUP(A29355,cordwood_density!A:D,4,FALSE)","v":1.258},{"v":0.739717669,"d":"0.74"}]
["37135","37","NC","135","Orange","","2104008100","Fireplace: general","Fireplace: general",6618.232458560001,"A","CEC Survey",2017,15,"I",1514.8842246385464,"TON",8,{"v":0.22889559019330002,"d":"0.23"},{"$f":"VLOOKUP(A29362,cordwood_density!A:D,4,FALSE)","v":1.1537},{"v":0.19840130900000003,"d":"0.20"}]
["37139","37","NC","139","Pasquotank","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",454.50901410139,"A","CEC Survey",2017,15,"I",190.75907098449937,"TON",8,{"v":0.41970360337440005,"d":"0.42"},{"$f":"VLOOKUP(A29394,cordwood_density!A:D,4,FALSE)","v":1.2471},{"v":0.336543664,"d":"0.34"}]
["37141","37","NC","141","Pender","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1213.8600089152599,"A","CEC Survey",2017,15,"I",1357.3188269819539,"TON",8,{"v":1.1181839891034,"d":"1.12"},{"$f":"VLOOKUP(A29415,cordwood_density!A:D,4,FALSE)","v":1.2462},{"v":0.897274907,"d":"0.90"}]
["37145","37","NC","145","Person","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",451.61849436179995,"A","CEC Survey",2017,15,"I",278.18569045434657,"TON",8,{"v":0.6159749742920999,"d":"0.62"},{"$f":"VLOOKUP(A29438,cordwood_density!A:D,4,FALSE)","v":1.2281},{"v":0.501567441,"d":"0.50"}]
["37147","37","NC","147","Pitt","","2104008620","Hydronic heater: indoor","Hydronic heater",94.78321433753047,"A","CEC Survey",2017,15,"I",166.63999353104305,"TON",8,{"v":1.7581171381002647,"d":"1.76"},{"$f":"VLOOKUP(A29450,cordwood_density!A:D,4,FALSE)","v":1.1857},{"v":1.4827672582442986,"d":"1.48"}]
["37149","37","NC","149","Polk","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1472.294225868,"A","CEC Survey",2017,15,"I",389.6586865990782,"TON",8,{"v":0.26466088078919997,"d":"0.26"},{"$f":"VLOOKUP(A29471,cordwood_density!A:D,4,FALSE)","v":1.4577},{"v":0.181560596,"d":"0.18"}]
["37155","37","NC","155","Robeson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1532.3204342635797,"A","CEC Survey",2017,15,"I",706.0273766441863,"TON",8,{"v":0.46075700673110004,"d":"0.46"},{"$f":"VLOOKUP(A29514,cordwood_density!A:D,4,FALSE)","v":1.2391},{"v":0.37184812100000003,"d":"0.37"}]
["37157","37","NC","157","Rockingham","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",969.8055858391,"A","CEC Survey",2017,15,"I",643.9232947975222,"TON",8,{"v":0.663971526046,"d":"0.66"},{"$f":"VLOOKUP(A29528,cordwood_density!A:D,4,FALSE)","v":1.3171},{"v":0.50411626,"d":"0.50"}]
["37159","37","NC","159","Rowan","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1663.7537317530803,"A","CEC Survey",2017,15,"I",1590.3377160937719,"TON",8,{"v":0.9558732676248001,"d":"0.96"},{"$f":"VLOOKUP(A29549,cordwood_density!A:D,4,FALSE)","v":1.1938},{"v":0.800697996,"d":"0.80"}]
["37161","37","NC","161","Rutherford","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1159.64128343112,"A","CEC Survey",2017,15,"I",1290.4627568142334,"TON",8,{"v":1.1128120180372,"d":"1.11"},{"$f":"VLOOKUP(A29566,cordwood_density!A:D,4,FALSE)","v":1.1908},{"v":0.934507909,"d":"0.93"}]
["37167","37","NC","167","Stanly","","2104008620","Hydronic heater: indoor","Hydronic heater",89.87606564045393,"A","CEC Survey",2017,15,"I",184.33821921725084,"TON",8,{"v":2.0510267989999638,"d":"2.05"},{"$f":"VLOOKUP(A29600,cordwood_density!A:D,4,FALSE)","v":1.3324},{"v":1.5393476425997927,"d":"1.54"}]
["37167","37","NC","167","Stanly","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",630.78570789696,"A","CEC Survey",2017,15,"I",377.67706784217904,"TON",8,{"v":0.5987406865976,"d":"0.60"},{"$f":"VLOOKUP(A29605,cordwood_density!A:D,4,FALSE)","v":1.3324},{"v":0.449370074,"d":"0.45"}]
["37173","37","NC","173","Swain","","2104008610","Hydronic heater: outdoor","Hydronic heater",75.32758509728285,"A","CEC Survey",2017,15,"I",189.25797175796924,"TON",8,{"v":2.5124656726158077,"d":"2.51"},{"$f":"VLOOKUP(A29644,cordwood_density!A:D,4,FALSE)","v":1.4391},{"v":1.7458589900742183,"d":"1.75"}]
["37173","37","NC","173","Swain","","2104009000","Wax Log; Total: All Combustor Types",null,78.47927997323498,"A","CEC Survey",2017,15,"I",10.987099196252899,"TON",8,0.14,{"$f":"VLOOKUP(A29653,cordwood_density!A:D,4,FALSE)","v":1.4391},{"v":0.09728302411229241,"d":"0.10"}]
["37177","37","NC","177","Tyrrell","","2104009000","Wax Log; Total: All Combustor Types",null,22.10461417986981,"A","CEC Survey",2017,15,"I",7.5913600170249635,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A29683,cordwood_density!A:D,4,FALSE)","v":1.086},{"v":0.31623273480662983,"d":"0.32"}]
["37181","37","NC","181","Vance","","2104008610","Hydronic heater: outdoor","Hydronic heater",93.31173305814454,"A","CEC Survey",2017,15,"I",178.39976777738678,"TON",8,{"v":1.911868549973475,"d":"1.91"},{"$f":"VLOOKUP(A29704,cordwood_density!A:D,4,FALSE)","v":1.2081},{"v":1.582541635604234,"d":"1.58"}]
["37183","37","NC","183","Wake","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",7006.48887347324,"A","CEC Survey",2017,15,"I",4861.360431008683,"TON",8,{"v":0.6938368873194001,"d":"0.69"},{"$f":"VLOOKUP(A29729,cordwood_density!A:D,4,FALSE)","v":1.1694},{"v":0.593327251,"d":"0.59"}]
["37185","37","NC","185","Warren","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",346.1513582426999,"A","CEC Survey",2017,15,"I",218.03387662431786,"TON",8,{"v":0.6298801707184,"d":"0.63"},{"$f":"VLOOKUP(A29739,cordwood_density!A:D,4,FALSE)","v":1.2178},{"v":0.517227928,"d":"0.52"}]
["37191","37","NC","191","Wayne","","2104008100","Fireplace: general","Fireplace: general",2724.5659417790002,"A","CEC Survey",2017,15,"I",853.3511681195399,"TON",8,{"v":0.3132062817912001,"d":"0.31"},{"$f":"VLOOKUP(A29782,cordwood_density!A:D,4,FALSE)","v":1.3201},{"v":0.23725951200000006,"d":"0.24"}]
["37193","37","NC","193","Wilkes","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1972.9879445358,"A","CEC Survey",2017,15,"I",2323.6147212104966,"TON",8,{"v":1.1777135930535,"d":"1.18"},{"$f":"VLOOKUP(A29805,cordwood_density!A:D,4,FALSE)","v":1.1995},{"v":0.9818370930000001,"d":"0.98"}]
["37195","37","NC","195","Wilson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",912.463769904,"A","CEC Survey",2017,15,"I",185.83012398038335,"TON",8,{"v":0.203657537,"d":"0.20"},{"$f":"VLOOKUP(A29817,cordwood_density!A:D,4,FALSE)","v":1.3036},{"v":0.15622701518870818,"d":"0.16"}]
["37199","37","NC","199","Yancey","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.14321053601433,"A","CEC Survey",2017,15,"I",18.105238832055036,"TON",8,{"v":2.2233538911934594,"d":"2.22"},{"$f":"VLOOKUP(A29838,cordwood_density!A:D,4,FALSE)","v":1.2904},{"v":1.7229958859217758,"d":"1.72"}]
["38001","38","ND","001","Adams","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",7.25597803104,"A","CEC Survey",2017,15,"I",0.4873553042097798,"TON",8,{"v":0.0671660391094,"d":"0.07"},{"$f":"VLOOKUP(A29858,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.051642349000000004,"d":"0.05"}]
["38003","38","ND","003","Barnes","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",168.739614588,"A","CEC Survey",2017,15,"I",26.30284342093457,"TON",8,{"v":0.155878295,"d":"0.16"},{"$f":"VLOOKUP(A29877,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.11985106489312625,"d":"0.12"}]
["38009","38","ND","009","Bottineau","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.8143935756634146,"A","CEC Survey",2017,15,"I",2.0227816794078524,"TON",8,{"v":0.5303022981984867,"d":"0.53"},{"$f":"VLOOKUP(A29916,cordwood_density!A:D,4,FALSE)","v":1.19},{"v":0.44563218336007293,"d":"0.45"}]
["38011","38","ND","011","Bowman","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",35.437475681920006,"A","CEC Survey",2017,15,"I",2.3790926356976985,"TON",8,{"v":0.06713493526039999,"d":"0.07"},{"$f":"VLOOKUP(A29934,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.05161843399999999,"d":"0.05"}]
["38013","38","ND","013","Burke","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",144.3979422961998,"A","CEC Survey",2017,15,"I",40.694047801517975,"TON",8,{"$f":"P29955/J29955","v":{"v":0.28181875139220003,"d":"0.28"}},{"$f":"VLOOKUP(A29955,cordwood_density!A:D,4,FALSE)","v":1.1946},{"$f":"S29955/T29955","v":{"v":0.235910557,"d":"0.24"}}]
["38017","38","ND","017","Cass","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",557.6864488358157,"A","CEC Survey",2017,15,"I",281.8434559411222,"TON",8,{"v":0.505379782007394,"d":"0.51"},{"$f":"VLOOKUP(A29972,cordwood_density!A:D,4,FALSE)","v":1.2052},{"v":0.41933270992979915,"d":"0.42"}]
["38019","38","ND","019","Cavalier","","2104008610","Hydronic heater: outdoor","Hydronic heater",64.01859964109792,"A","CEC Survey",2017,15,"I",36.68759053439445,"TON",8,{"v":0.5730770547945909,"d":"0.57"},{"$f":"VLOOKUP(A29989,cordwood_density!A:D,4,FALSE)","v":1.2888},{"v":0.4446594155761879,"d":"0.44"}]
["38023","38","ND","023","Divide","","2104008620","Hydronic heater: indoor","Hydronic heater",27.666207373565804,"A","CEC Survey",2017,15,"I",15.186933805786532,"TON",8,{"v":0.5489344311174784,"d":"0.55"},{"$f":"VLOOKUP(A30020,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.44268905735280517,"d":"0.44"}]
["38027","38","ND","027","Eddy","","2104008620","Hydronic heater: indoor","Hydronic heater",18.87537310792378,"A","CEC Survey",2017,15,"I",10.562999241729441,"TON",8,{"v":0.5596180367579144,"d":"0.56"},{"$f":"VLOOKUP(A30050,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.4302768235875092,"d":"0.43"}]
["38029","38","ND","029","Emmons","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,244.85897978,"A","CEC Survey",2017,15,"I",12.765745131537857,"TON",8,{"v":0.052135090749,"d":"0.05"},{"$f":"VLOOKUP(A30071,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.040085415000000006,"d":"0.04"}]
["38029","38","ND","029","Emmons","","2104009000","Wax Log; Total: All Combustor Types",null,25.105448864386755,"A","CEC Survey",2017,15,"I",19.59466224814022,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A30073,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.6001033369214208,"d":"0.60"}]
["38033","38","ND","033","Golden Valley","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",54.4523585508,"A","CEC Survey",2017,15,"I",16.27463869958888,"TON",8,{"v":0.29887848998140004,"d":"0.30"},{"$f":"VLOOKUP(A30106,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.22980046900000003,"d":"0.23"}]
["38037","38","ND","037","Grant","","2104008100","Fireplace: general","Fireplace: general",36.59147745,"A","CEC Survey",2017,15,"I",2.9440896358134268,"TON",8,{"v":0.08045834278859999,"d":"0.08"},{"$f":"VLOOKUP(A30127,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.061862481,"d":"0.06"}]
["38039","38","ND","039","Griggs","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",36.25557862932,"A","CEC Survey",2017,15,"I",10.911867403879748,"TON",8,{"v":0.300970714478,"d":"0.30"},{"$f":"VLOOKUP(A30149,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.23140913000000002,"d":"0.23"}]
["38041","38","ND","041","Hettinger","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",75.01788665139999,"A","CEC Survey",2017,15,"I",21.22882868530324,"TON",8,{"v":0.28298356076,"d":"0.28"},{"$f":"VLOOKUP(A30166,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.228212549,"d":"0.23"}]
["38047","38","ND","047","Logan","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",22.034139427649997,"A","CEC Survey",2017,15,"I",1.4911246851412994,"TON",8,{"v":0.0676733797586,"d":"0.07"},{"$f":"VLOOKUP(A30205,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.052032431,"d":"0.05"}]
["38049","38","ND","049","McHenry","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",413.98913921101,"A","CEC Survey",2017,15,"I",100.37868245623734,"TON",8,{"v":0.24246694647,"d":"0.24"},{"$f":"VLOOKUP(A30225,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.23841391000000003,"d":"0.24"}]
["38053","38","ND","053","Mckenzie","","2104008610","Hydronic heater: outdoor","Hydronic heater",81.82051205820582,"A","CEC Survey",2017,15,"I",43.77567594434487,"TON",8,{"v":0.5350208015467264,"d":"0.54"},{"$f":"VLOOKUP(A30244,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.43254976275101165,"d":"0.43"}]
["38055","38","ND","055","Mclean","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.207609495086156,"A","CEC Survey",2017,15,"I",1.671698268308594,"TON",8,{"v":0.5211663922523999,"d":"0.52"},{"$f":"VLOOKUP(A30261,cordwood_density!A:D,4,FALSE)","v":1.2126},{"v":0.4297925055685304,"d":"0.43"}]
["38057","38","ND","057","Mercer","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",27.7860760602,"A","CEC Survey",2017,15,"I",1.7501888698449393,"TON",8,{"v":0.06298798240000002,"d":"0.06"},{"$f":"VLOOKUP(A30278,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.05079676000000002,"d":"0.05"}]
["38059","38","ND","059","Morton","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",807.77786136034,"A","CEC Survey",2017,15,"I",145.72464714787827,"TON",8,{"v":0.18040188289200002,"d":"0.18"},{"$f":"VLOOKUP(A30300,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":0.195240133,"d":"0.20"}]
["38065","38","ND","065","Oliver","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",29.001515484080002,"A","CEC Survey",2017,15,"I",1.9411614970406879,"TON",8,{"$f":"P30339/J30339","v":{"v":0.0669331055512,"d":"0.07"}},{"$f":"VLOOKUP(A30339,cordwood_density!A:D,4,FALSE)","v":1.3006},{"$f":"S30339/T30339","v":{"v":0.051463251999999994,"d":"0.05"}}]
["38065","38","ND","065","Oliver","","2104009000","Wax Log; Total: All Combustor Types",null,12.640954444176845,"A","CEC Survey",2017,15,"I",9.866194154335139,"TON",8,{"v":0.7804943999999998,"d":"0.78"},{"$f":"VLOOKUP(A30343,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.6001033369214207,"d":"0.60"}]
["38071","38","ND","071","Ramsey","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.099744408181909,"A","CEC Survey",2017,15,"I",3.227371616759383,"TON",8,{"v":0.5290994836489115,"d":"0.53"},{"$f":"VLOOKUP(A30378,cordwood_density!A:D,4,FALSE)","v":1.2214},{"v":0.4331909969288615,"d":"0.43"}]
["38073","38","ND","073","Ransom","","2104008620","Hydronic heater: indoor","Hydronic heater",49.656071344989805,"A","CEC Survey",2017,15,"I",26.906763189939756,"TON",8,{"v":0.5418625046472709,"d":"0.54"},{"$f":"VLOOKUP(A30395,cordwood_density!A:D,4,FALSE)","v":1.2582},{"v":0.4306648423519877,"d":"0.43"}]
["38075","38","ND","075","Renville","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,156.26552537700002,"A","CEC Survey",2017,15,"I",8.085733075844809,"TON",8,{"v":0.051743550321399996,"d":"0.05"},{"$f":"VLOOKUP(A30416,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.039784369,"d":"0.04"}]
["38079","38","ND","079","Rolette","","2104008620","Hydronic heater: indoor","Hydronic heater",122.66621206495822,"A","CEC Survey",2017,15,"I",71.38499370160258,"TON",8,{"v":0.5819450401207503,"d":"0.58"},{"$f":"VLOOKUP(A30440,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.4474435184689761,"d":"0.45"}]
["38081","38","ND","081","Sargent","","2104008620","Hydronic heater: indoor","Hydronic heater",37.57442482154085,"A","CEC Survey",2017,15,"I",21.216784769392685,"TON",8,{"v":0.5646602674601534,"d":"0.56"},{"$f":"VLOOKUP(A30455,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.43415367327399157,"d":"0.43"}]
["38085","38","ND","085","Sioux","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",36.79103302344,"A","CEC Survey",2017,15,"I",7.874719201418847,"TON",8,{"v":0.214039089264,"d":"0.21"},{"$f":"VLOOKUP(A30494,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":0.231644036,"d":"0.23"}]
["38089","38","ND","089","Stark","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.369459091328843,"A","CEC Survey",2017,15,"I",1.5729237682189408,"TON",8,{"v":0.46681788547805547,"d":"0.47"},{"$f":"VLOOKUP(A30516,cordwood_density!A:D,4,FALSE)","v":1.1208},{"v":0.4165041804764949,"d":"0.42"}]
["38091","38","ND","091","Steele","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",8.015360024640001,"A","CEC Survey",2017,15,"I",0.5276017068722032,"TON",8,{"v":0.06582383139999999,"d":"0.07"},{"$f":"VLOOKUP(A30533,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.05308373499999999,"d":"0.05"}]
["38093","38","ND","093","Stutsman","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",119.41646754516853,"A","CEC Survey",2017,15,"I",7.47204824128199,"TON",8,{"v":0.06257133873479999,"d":"0.06"},{"$f":"VLOOKUP(A30550,cordwood_density!A:D,4,FALSE)","v":1.2076},{"v":0.05181462299999999,"d":"0.05"}]
["38095","38","ND","095","Towner","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",34.661005362599994,"A","CEC Survey",2017,15,"I",10.617002545763926,"TON",8,{"v":0.3063097112936,"d":"0.31"},{"$f":"VLOOKUP(A30569,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.23551415600000003,"d":"0.24"}]
["38099","38","ND","099","Walsh","","2104008610","Hydronic heater: outdoor","Hydronic heater",125.57948207882455,"A","CEC Survey",2017,15,"I",66.79897600907593,"TON",8,{"v":0.53192587597349,"d":"0.53"},{"$f":"VLOOKUP(A30589,cordwood_density!A:D,4,FALSE)","v":1.2159},{"v":0.43747501930544447,"d":"0.44"}]
["38103","38","ND","103","Wells","","2104009000","Wax Log; Total: All Combustor Types",null,31.89113889297528,"A","CEC Survey",2017,15,"I",24.890855315589405,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A30628,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.6001033369214208,"d":"0.60"}]
["38105","38","ND","105","Williams","","2104008610","Hydronic heater: outdoor","Hydronic heater",143.60461135001583,"A","CEC Survey",2017,15,"I",79.20402909521724,"TON",8,{"v":0.5515423798067923,"d":"0.55"},{"$f":"VLOOKUP(A30634,cordwood_density!A:D,4,FALSE)","v":1.2731},{"v":0.43322785311978035,"d":"0.43"}]
["39003","39","OH","003","Allen","","2104008100","Fireplace: general","Fireplace: general",3436.617664153,"A","CEC Survey",2017,15,"I",1442.5913136807394,"TON",8,{"v":0.4197706741509999,"d":"0.42"},{"$f":"VLOOKUP(A30667,cordwood_density!A:D,4,FALSE)","v":1.3334},{"v":0.3148122649999999,"d":"0.31"}]
["39005","39","OH","005","Ashland","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",572.18276367208,"A","CEC Survey",2017,15,"I",380.66203296752303,"TON",8,{"v":0.6652804962606,"d":"0.67"},{"$f":"VLOOKUP(A30684,cordwood_density!A:D,4,FALSE)","v":1.3222},{"v":0.503161773,"d":"0.50"}]
["39009","39","OH","009","Athens","","2104008620","Hydronic heater: indoor","Hydronic heater",108.51077613176822,"A","CEC Survey",2017,15,"I",334.2862276132085,"TON",8,{"v":3.080673086397186,"d":"3.08"},{"$f":"VLOOKUP(A30710,cordwood_density!A:D,4,FALSE)","v":1.3229},{"v":2.3287271043897393,"d":"2.33"}]
["39011","39","OH","011","Auglaize","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",9.314083452812788,"A","CEC Survey",2017,15,"I",28.391080697694747,"TON",8,{"$f":"P30723/J30723","v":{"v":3.0481883527810605,"d":"3.05"}},{"$f":"VLOOKUP(A30723,cordwood_density!A:D,4,FALSE)","v":1.3333},{"$f":"S30723/T30723","v":{"v":2.286198419546284,"d":"2.29"}}]
["39015","39","OH","015","Brown","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",672.275519376,"A","CEC Survey",2017,15,"I",421.7785569210892,"TON",8,{"v":0.627389433,"d":"0.63"},{"$f":"VLOOKUP(A30762,cordwood_density!A:D,4,FALSE)","v":1.3688},{"v":0.4583499656633548,"d":"0.46"}]
["39019","39","OH","019","Carroll","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.66926388744467,"A","CEC Survey",2017,15,"I",33.3357643644627,"TON",8,{"v":3.1244671343907253,"d":"3.12"},{"$f":"VLOOKUP(A30783,cordwood_density!A:D,4,FALSE)","v":1.2878},{"v":2.426205260436966,"d":"2.43"}]
["39021","39","OH","021","Champaign","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",625.267018334,"A","CEC Survey",2017,15,"I",305.6127015779718,"TON",8,{"v":0.48877150500000005,"d":"0.49"},{"$f":"VLOOKUP(A30807,cordwood_density!A:D,4,FALSE)","v":1.3688},{"v":0.3570802929573349,"d":"0.36"}]
["39023","39","OH","023","Clark","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1605.3011978959998,"A","CEC Survey",2017,15,"I",588.8367246257903,"TON",8,{"v":0.36680762800000005,"d":"0.37"},{"$f":"VLOOKUP(A30822,cordwood_density!A:D,4,FALSE)","v":1.3698},{"v":0.26778188640677475,"d":"0.27"}]
["39025","39","OH","025","Clermont","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",876.60692315424,"A","CEC Survey",2017,15,"I",1272.3301093422695,"TON",8,{"v":1.4514260334200002,"d":"1.45"},{"$f":"VLOOKUP(A30839,cordwood_density!A:D,4,FALSE)","v":1.3765},{"v":1.05443228,"d":"1.05"}]
["39029","39","OH","029","Columbiana","","2104008620","Hydronic heater: indoor","Hydronic heater",209.70403316824496,"A","CEC Survey",2017,15,"I",639.574218173935,"TON",8,{"v":3.049889925869029,"d":"3.05"},{"$f":"VLOOKUP(A30860,cordwood_density!A:D,4,FALSE)","v":1.3223},{"v":2.3065037630409355,"d":"2.31"}]
["39031","39","OH","031","Coshocton","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",117.47469602376,"A","CEC Survey",2017,15,"I",98.65209323397418,"TON",8,{"v":0.8397731304963,"d":"0.84"},{"$f":"VLOOKUP(A30878,cordwood_density!A:D,4,FALSE)","v":1.2879},{"v":0.652048397,"d":"0.65"}]
["39037","39","OH","037","Darke","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",176.44402790682992,"A","CEC Survey",2017,15,"I",560.6069667205278,"TON",8,{"v":3.177251014789532,"d":"3.18"},{"$f":"VLOOKUP(A30917,cordwood_density!A:D,4,FALSE)","v":1.3687},{"v":2.321364078899344,"d":"2.32"}]
["39037","39","OH","037","Darke","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",387.67884467445,"A","CEC Survey",2017,15,"I",196.30480541070162,"TON",8,{"v":0.5063593438418,"d":"0.51"},{"$f":"VLOOKUP(A30925,cordwood_density!A:D,4,FALSE)","v":1.3687},{"v":0.369956414,"d":"0.37"}]
["39041","39","OH","041","Delaware","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,9107.324900853,"A","CEC Survey",2017,15,"I",3155.8600534847737,"TON",8,{"v":0.34651888318920004,"d":"0.35"},{"$f":"VLOOKUP(A30956,cordwood_density!A:D,4,FALSE)","v":1.3341},{"v":0.259739812,"d":"0.26"}]
["39043","39","OH","043","Erie","","2104009000","Wax Log; Total: All Combustor Types",null,506.55256152762973,"A","CEC Survey",2017,15,"I",282.60531720491946,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A30973,cordwood_density!A:D,4,FALSE)","v":1.3246},{"v":0.4211832217197644,"d":"0.42"}]
["39047","39","OH","047","Fayette","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1609.8596373730002,"A","CEC Survey",2017,15,"I",530.5225957859958,"TON",8,{"v":0.3295458706274,"d":"0.33"},{"$f":"VLOOKUP(A31001,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.253379879,"d":"0.25"}]
["39049","39","OH","049","Franklin","","2104008100","Fireplace: general","Fireplace: general",51589.99243202,"A","CEC Survey",2017,15,"I",10907.683167554655,"TON",8,{"v":0.211430214531,"d":"0.21"},{"$f":"VLOOKUP(A31012,cordwood_density!A:D,4,FALSE)","v":1.383},{"v":0.152877957,"d":"0.15"}]
["39053","39","OH","053","Gallia","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",643.224528576,"A","CEC Survey",2017,15,"I",1232.3821782466257,"TON",8,{"v":1.9159440032159998,"d":"1.92"},{"$f":"VLOOKUP(A31051,cordwood_density!A:D,4,FALSE)","v":1.368},{"v":1.4005438619999997,"d":"1.40"}]
["39057","39","OH","057","Greene","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1751.60477976,"A","CEC Survey",2017,15,"I",596.6194569382606,"TON",8,{"v":0.340613056,"d":"0.34"},{"$f":"VLOOKUP(A31077,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.2487497670342511,"d":"0.25"}]
["39059","39","OH","059","Guernsey","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",386.14494833774995,"A","CEC Survey",2017,15,"I",322.3853620344489,"TON",8,{"v":0.834881728797,"d":"0.83"},{"$f":"VLOOKUP(A31090,cordwood_density!A:D,4,FALSE)","v":1.2879},{"v":0.6482504299999999,"d":"0.65"}]
["39061","39","OH","061","Hamilton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",6011.401140404099,"A","CEC Survey",2017,15,"I",6330.556432387331,"TON",8,{"v":1.0530916644105002,"d":"1.05"},{"$f":"VLOOKUP(A31111,cordwood_density!A:D,4,FALSE)","v":1.3715},{"v":0.7678393470000001,"d":"0.77"}]
["39065","39","OH","065","Hardin","","2104008620","Hydronic heater: indoor","Hydronic heater",51.027420789186046,"A","CEC Survey",2017,15,"I",156.50933153390758,"TON",8,{"v":3.0671613245064453,"d":"3.07"},{"$f":"VLOOKUP(A31130,cordwood_density!A:D,4,FALSE)","v":1.3326},{"v":2.301636893671353,"d":"2.30"}]
["39067","39","OH","067","Harrison","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.246700096064758,"A","CEC Survey",2017,15,"I",7.162845546245192,"TON",8,{"v":3.1881627453487824,"d":"3.19"},{"$f":"VLOOKUP(A31146,cordwood_density!A:D,4,FALSE)","v":1.3124},{"v":2.4292614639963293,"d":"2.43"}]
["39069","39","OH","069","Henry","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",463.1833752,"A","CEC Survey",2017,15,"I",191.10541840620462,"TON",8,{"v":0.412591273,"d":"0.41"},{"$f":"VLOOKUP(A31167,cordwood_density!A:D,4,FALSE)","v":1.392},{"v":0.2964017765804598,"d":"0.30"}]
["39075","39","OH","075","Holmes","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.30675488278174,"A","CEC Survey",2017,15,"I",13.090407815404612,"TON",8,{"v":3.0395061181075382,"d":"3.04"},{"$f":"VLOOKUP(A31206,cordwood_density!A:D,4,FALSE)","v":1.288},{"v":2.359864998530697,"d":"2.36"}]
["39077","39","OH","077","Huron","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",783.3062892759999,"A","CEC Survey",2017,15,"I",380.7359988748063,"TON",8,{"v":0.486062737,"d":"0.49"},{"$f":"VLOOKUP(A31227,cordwood_density!A:D,4,FALSE)","v":1.3223},{"v":0.36758885048778644,"d":"0.37"}]
["39079","39","OH","079","Jackson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",952.1624330864801,"A","CEC Survey",2017,15,"I",1744.984055126046,"TON",8,{"v":1.8326537515974,"d":"1.83"},{"$f":"VLOOKUP(A31245,cordwood_density!A:D,4,FALSE)","v":1.3681},{"v":1.339561254,"d":"1.34"}]
["39083","39","OH","083","Knox","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",208.5080094647738,"A","CEC Survey",2017,15,"I",643.2972207880634,"TON",8,{"v":3.0852398545234045,"d":"3.09"},{"$f":"VLOOKUP(A31262,cordwood_density!A:D,4,FALSE)","v":1.3343},{"v":2.3122535070999057,"d":"2.31"}]
["39087","39","OH","087","Lawrence","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",194.37188164703727,"A","CEC Survey",2017,15,"I",616.8777092593795,"TON",8,{"v":3.173698294383838,"d":"3.17"},{"$f":"VLOOKUP(A31292,cordwood_density!A:D,4,FALSE)","v":1.3672},{"v":2.3213123861789335,"d":"2.32"}]
["39087","39","OH","087","Lawrence","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3599.04274807,"A","CEC Survey",2017,15,"I",1255.5312426743114,"TON",8,{"v":0.34885143927440004,"d":"0.35"},{"$f":"VLOOKUP(A31301,cordwood_density!A:D,4,FALSE)","v":1.3672},{"v":0.255157577,"d":"0.26"}]
["39093","39","OH","093","Lorain","","2104008620","Hydronic heater: indoor","Hydronic heater",329.44939742976163,"A","CEC Survey",2017,15,"I",913.6912779173977,"TON",8,{"v":2.773388827072285,"d":"2.77"},{"$f":"VLOOKUP(A31340,cordwood_density!A:D,4,FALSE)","v":1.3216},{"v":2.098508495060748,"d":"2.10"}]
["39093","39","OH","093","Lorain","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1592.0096035704,"A","CEC Survey",2017,15,"I",983.5471721904978,"TON",8,{"v":0.6178022858560002,"d":"0.62"},{"$f":"VLOOKUP(A31345,cordwood_density!A:D,4,FALSE)","v":1.3216},{"v":0.4674654100000001,"d":"0.47"}]
["39097","39","OH","097","Madison","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",184.99264594272,"A","CEC Survey",2017,15,"I",295.56888802681306,"TON",8,{"v":1.5977331775573997,"d":"1.60"},{"$f":"VLOOKUP(A31379,cordwood_density!A:D,4,FALSE)","v":1.3754},{"v":1.1616498309999999,"d":"1.16"}]
["39101","39","OH","101","Marion","","2104008620","Hydronic heater: indoor","Hydronic heater",74.5735844522765,"A","CEC Survey",2017,15,"I",219.20729768278352,"TON",8,{"v":2.9394764820922026,"d":"2.94"},{"$f":"VLOOKUP(A31400,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":2.2035056087647695,"d":"2.20"}]
["39103","39","OH","103","Medina","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,9522.408379384,"A","CEC Survey",2017,15,"I",3273.280875881963,"TON",8,{"v":0.343745063798,"d":"0.34"},{"$f":"VLOOKUP(A31421,cordwood_density!A:D,4,FALSE)","v":1.322},{"v":0.260018959,"d":"0.26"}]
["39105","39","OH","105","Meigs","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",275.0950779326221,"A","CEC Survey",2017,15,"I",249.22873740854368,"TON",8,{"v":0.9059730885828,"d":"0.91"},{"$f":"VLOOKUP(A31435,cordwood_density!A:D,4,FALSE)","v":1.3228},{"v":0.684890451,"d":"0.68"}]
["39111","39","OH","111","Monroe","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",52.00995203712,"A","CEC Survey",2017,15,"I",53.015005999647094,"TON",8,{"v":1.0193242624375,"d":"1.02"},{"$f":"VLOOKUP(A31478,cordwood_density!A:D,4,FALSE)","v":1.2875},{"v":0.791708165,"d":"0.79"}]
["39113","39","OH","113","Montgomery","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",5065.159488435,"A","CEC Survey",2017,15,"I",2402.0213987515576,"TON",8,{"v":0.474224238,"d":"0.47"},{"$f":"VLOOKUP(A31497,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.36461958942026756,"d":"0.36"}]
["39115","39","OH","115","Morgan","","2104009000","Wax Log; Total: All Combustor Types",null,98.11177332561621,"A","CEC Survey",2017,15,"I",54.73648921763586,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A31513,cordwood_density!A:D,4,FALSE)","v":1.3221},{"v":0.42197965017018374,"d":"0.42"}]
["39119","39","OH","119","Muskingum","","2104008610","Hydronic heater: outdoor","Hydronic heater",232.91426493677244,"A","CEC Survey",2017,15,"I",677.0311120330155,"TON",8,{"v":2.906782511654253,"d":"2.91"},{"$f":"VLOOKUP(A31534,cordwood_density!A:D,4,FALSE)","v":1.288},{"v":2.2568187202284573,"d":"2.26"}]
["39121","39","OH","121","Noble","","2104008620","Hydronic heater: indoor","Hydronic heater",34.14219426857346,"A","CEC Survey",2017,15,"I",102.77710720503563,"TON",8,{"v":3.0102666043241952,"d":"3.01"},{"$f":"VLOOKUP(A31550,cordwood_density!A:D,4,FALSE)","v":1.2884},{"v":2.3364379108384004,"d":"2.34"}]
["39123","39","OH","123","Ottawa","","2104009000","Wax Log; Total: All Combustor Types",null,280.6516472092308,"A","CEC Survey",2017,15,"I",156.5753562561379,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A31573,cordwood_density!A:D,4,FALSE)","v":1.3321},{"v":0.41881187259965463,"d":"0.42"}]
["39129","39","OH","129","Pickaway","","2104008100","Fireplace: general","Fireplace: general",1442.67253374,"A","CEC Survey",2017,15,"I",712.4165982590328,"TON",8,{"v":0.49381726039529994,"d":"0.49"},{"$f":"VLOOKUP(A31612,cordwood_density!A:D,4,FALSE)","v":1.3693},{"v":0.36063482099999994,"d":"0.36"}]
["39131","39","OH","131","Pike","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",492.37248146636,"A","CEC Survey",2017,15,"I",442.2903004336621,"TON",8,{"v":0.8982839559117001,"d":"0.90"},{"$f":"VLOOKUP(A31629,cordwood_density!A:D,4,FALSE)","v":1.3551},{"v":0.6628912670000001,"d":"0.66"}]
["39131","39","OH","131","Pike","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",590.1768818406999,"A","CEC Survey",2017,15,"I",1102.3560721626377,"TON",8,{"v":1.8678401443385997,"d":"1.87"},{"$f":"VLOOKUP(A31636,cordwood_density!A:D,4,FALSE)","v":1.3551},{"v":1.378378086,"d":"1.38"}]
["39137","39","OH","137","Putnam","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.427449741719634,"A","CEC Survey",2017,15,"I",35.375983149861476,"TON",8,{"v":3.095702361368513,"d":"3.10"},{"$f":"VLOOKUP(A31668,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":2.3802109498450816,"d":"2.38"}]
["39139","39","OH","139","Richland","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1167.03332460869,"A","CEC Survey",2017,15,"I",789.2116863426435,"TON",8,{"v":0.6762546276107999,"d":"0.68"},{"$f":"VLOOKUP(A31689,cordwood_density!A:D,4,FALSE)","v":1.3223},{"v":0.511422996,"d":"0.51"}]
["39143","39","OH","143","Sandusky","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",149.35612640325286,"A","CEC Survey",2017,15,"I",448.2719187902476,"TON",8,{"v":3.0013627802581024,"d":"3.00"},{"$f":"VLOOKUP(A31712,cordwood_density!A:D,4,FALSE)","v":1.3331},{"v":2.2514160830081034,"d":"2.25"}]
["39147","39","OH","147","Seneca","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.021345886931424,"A","CEC Survey",2017,15,"I",12.259170657977442,"TON",8,{"v":3.0485243007365557,"d":"3.05"},{"$f":"VLOOKUP(A31746,cordwood_density!A:D,4,FALSE)","v":1.3322},{"v":2.2883383131185675,"d":"2.29"}]
["39149","39","OH","149","Shelby","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",658.499128185,"A","CEC Survey",2017,15,"I",282.62644099333545,"TON",8,{"v":0.42919789700000005,"d":"0.43"},{"$f":"VLOOKUP(A31767,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.329999920805782,"d":"0.33"}]
["39153","39","OH","153","Summit","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",75.43576120855839,"A","CEC Survey",2017,15,"I",87.22095264199312,"TON",8,{"v":1.1562281767244589,"d":"1.16"},{"$f":"VLOOKUP(A31788,cordwood_density!A:D,4,FALSE)","v":1.3221},{"v":0.8745391246686778,"d":"0.87"}]
["39155","39","OH","155","Trumbull","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",529.9726029534406,"A","CEC Survey",2017,15,"I",1527.7902553419997,"TON",8,{"v":2.8827721411029614,"d":"2.88"},{"$f":"VLOOKUP(A31802,cordwood_density!A:D,4,FALSE)","v":1.3221},{"v":2.180449391954437,"d":"2.18"}]
["39157","39","OH","157","Tuscarawas","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",235.53732845075393,"A","CEC Survey",2017,15,"I",185.8510357873526,"TON",8,{"v":0.7890513024402002,"d":"0.79"},{"$f":"VLOOKUP(A31823,cordwood_density!A:D,4,FALSE)","v":1.2879},{"v":0.612665038,"d":"0.61"}]
["39159","39","OH","159","Union","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2766.19503237,"A","CEC Survey",2017,15,"I",946.0218010683783,"TON",8,{"v":0.341993890524,"d":"0.34"},{"$f":"VLOOKUP(A31841,cordwood_density!A:D,4,FALSE)","v":1.3332},{"v":0.25652107,"d":"0.26"}]
["39163","39","OH","163","Vinton","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",72.46092521175426,"A","CEC Survey",2017,15,"I",243.08680664163873,"TON",8,{"v":3.3547295446650796,"d":"3.35"},{"$f":"VLOOKUP(A31862,cordwood_density!A:D,4,FALSE)","v":1.3229},{"v":2.535890501674412,"d":"2.54"}]
["39167","39","OH","167","Washington","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3872.61377184,"A","CEC Survey",2017,15,"I",1309.435652826113,"TON",8,{"v":0.3381270970908,"d":"0.34"},{"$f":"VLOOKUP(A31901,cordwood_density!A:D,4,FALSE)","v":1.3227},{"v":0.255634004,"d":"0.26"}]
["39169","39","OH","169","Wayne","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1439.218847628,"A","CEC Survey",2017,15,"I",651.0621271975989,"TON",8,{"v":0.45237187400000006,"d":"0.45"},{"$f":"VLOOKUP(A31917,cordwood_density!A:D,4,FALSE)","v":1.3227},{"v":0.34200640659257586,"d":"0.34"}]
["39173","39","OH","173","Wood","","2104008620","Hydronic heater: indoor","Hydronic heater",135.92994687075029,"A","CEC Survey",2017,15,"I",406.5629037667004,"TON",8,{"v":2.990973756160465,"d":"2.99"},{"$f":"VLOOKUP(A31940,cordwood_density!A:D,4,FALSE)","v":1.3343},{"v":2.2416051533841452,"d":"2.24"}]
["39175","39","OH","175","Wyandot","","2104008100","Fireplace: general","Fireplace: general",631.4962695700368,"A","CEC Survey",2017,15,"I",304.8324066582711,"TON",8,{"v":0.48271450101490004,"d":"0.48"},{"$f":"VLOOKUP(A31957,cordwood_density!A:D,4,FALSE)","v":1.3321},{"v":0.362371069,"d":"0.36"}]
["40001","40","OK","001","Adair","","2104008620","Hydronic heater: indoor","Hydronic heater",34.774965166801024,"A","CEC Survey",2017,15,"I",91.72631729347181,"TON",8,{"v":2.6377112630738484,"d":"2.64"},{"$f":"VLOOKUP(A31970,cordwood_density!A:D,4,FALSE)","v":1.4572},{"v":1.8101230188538624,"d":"1.81"}]
["40003","40","OK","003","Alfalfa","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",71.07396652664,"A","CEC Survey",2017,15,"I",93.41971147983966,"TON",8,{"v":1.314401264559,"d":"1.31"},{"$f":"VLOOKUP(A31996,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.018442015,"d":"1.02"}]
["40009","40","OK","009","Beckham","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",93.88559381831742,"A","CEC Survey",2017,15,"I",37.40115107477127,"TON",8,{"v":0.3983694361794,"d":"0.40"},{"$f":"VLOOKUP(A32035,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.308669949,"d":"0.31"}]
["40011","40","OK","011","Blaine","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",112.63836415944002,"A","CEC Survey",2017,15,"I",143.15598760432272,"TON",8,{"v":1.270934540577,"d":"1.27"},{"$f":"VLOOKUP(A32056,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.984762545,"d":"0.98"}]
["40015","40","OK","015","Caddo","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",246.39756383366998,"A","CEC Survey",2017,15,"I",101.05006988876141,"TON",8,{"v":0.4101098578920001,"d":"0.41"},{"$f":"VLOOKUP(A32079,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.3177668200000001,"d":"0.32"}]
["40017","40","OK","017","Canadian","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.1437046585314,"A","CEC Survey",2017,15,"I",6.84025074789517,"TON",8,{"v":2.1758566694018366,"d":"2.18"},{"$f":"VLOOKUP(A32091,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.6859264446008342,"d":"1.69"}]
["40019","40","OK","019","Carter","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",656.5978523,"A","CEC Survey",2017,15,"I",144.15262971848028,"TON",8,{"v":0.219544778,"d":"0.22"},{"$f":"VLOOKUP(A32112,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.17011062916472958,"d":"0.17"}]
["40023","40","OK","023","Choctaw","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",31.27275604463742,"A","CEC Survey",2017,15,"I",79.03221474205233,"TON",8,{"v":2.5271905881670635,"d":"2.53"},{"$f":"VLOOKUP(A32132,cordwood_density!A:D,4,FALSE)","v":1.4091},{"v":1.7934785239990516,"d":"1.79"}]
["40025","40","OK","025","Cimarron","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.16659547359648808,"A","CEC Survey",2017,15,"I",0.3845734266451368,"TON",8,{"v":2.308426623742578,"d":"2.31"},{"$f":"VLOOKUP(A32151,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.7886460744944817,"d":"1.79"}]
["40029","40","OK","029","Coal","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",120.76678510400001,"A","CEC Survey",2017,15,"I",167.0315090630348,"TON",8,{"v":1.3830914594538,"d":"1.38"},{"$f":"VLOOKUP(A32190,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.071665473,"d":"1.07"}]
["40033","40","OK","033","Cotton","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.7570347145234342,"A","CEC Survey",2017,15,"I",1.6938642289113155,"TON",8,{"v":2.2374987519266285,"d":"2.24"},{"$f":"VLOOKUP(A32208,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.7336887896533617,"d":"1.73"}]
["40035","40","OK","035","Craig","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",134.31933332028578,"A","CEC Survey",2017,15,"I",56.33329618941623,"TON",8,{"v":0.4193982712458,"d":"0.42"},{"$f":"VLOOKUP(A32229,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.324963793,"d":"0.32"}]
["40037","40","OK","037","Creek","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3869.932307498,"A","CEC Survey",2017,15,"I",1067.751912285009,"TON",8,{"v":0.2759097129984,"d":"0.28"},{"$f":"VLOOKUP(A32246,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.213784064,"d":"0.21"}]
["40039","40","OK","039","Custer","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1314.3144417479998,"A","CEC Survey",2017,15,"I",358.3436165719964,"TON",8,{"v":0.2726467922664,"d":"0.27"},{"$f":"VLOOKUP(A32261,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.211255844,"d":"0.21"}]
["40043","40","OK","043","Dewey","","2104008620","Hydronic heater: indoor","Hydronic heater",7.234960448311808,"A","CEC Survey",2017,15,"I",16.88048059204716,"TON",8,{"v":2.3331821525003664,"d":"2.33"},{"$f":"VLOOKUP(A32285,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.807827485278449,"d":"1.81"}]
["40047","40","OK","047","Garfield","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",516.94735822672,"A","CEC Survey",2017,15,"I",553.3510656634539,"TON",8,{"v":1.0704205309446,"d":"1.07"},{"$f":"VLOOKUP(A32324,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.829397591,"d":"0.83"}]
["40051","40","OK","051","Grady","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",490.76236898283,"A","CEC Survey",2017,15,"I",211.93824959722878,"TON",8,{"v":0.43185513599280007,"d":"0.43"},{"$f":"VLOOKUP(A32349,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.3346157880000001,"d":"0.33"}]
["40053","40","OK","053","Grant","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",29.98589079969,"A","CEC Survey",2017,15,"I",11.142339355242305,"TON",8,{"v":0.37158607125180004,"d":"0.37"},{"$f":"VLOOKUP(A32363,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.287917303,"d":"0.29"}]
["40055","40","OK","055","Greer","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",24.605129666880003,"A","CEC Survey",2017,15,"I",9.882415771029732,"TON",8,{"v":0.40164046704179995,"d":"0.40"},{"$f":"VLOOKUP(A32380,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.311204453,"d":"0.31"}]
["40059","40","OK","059","Harper","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",9.1879187982802,"A","CEC Survey",2017,15,"I",21.505607434482133,"TON",8,{"v":2.340639692909298,"d":"2.34"},{"$f":"VLOOKUP(A32402,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.8136058367498047,"d":"1.81"}]
["40061","40","OK","061","Haskell","","2104008610","Hydronic heater: outdoor","Hydronic heater",27.66051245758288,"A","CEC Survey",2017,15,"I",70.80481540126945,"TON",8,{"v":2.5597795959076293,"d":"2.56"},{"$f":"VLOOKUP(A32419,cordwood_density!A:D,4,FALSE)","v":1.4109},{"v":1.814288465452994,"d":"1.81"}]
["40063","40","OK","063","Hughes","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",93.92551128386141,"A","CEC Survey",2017,15,"I",58.412615103960725,"TON",8,{"v":0.62190361602,"d":"0.62"},{"$f":"VLOOKUP(A32440,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.4818717,"d":"0.48"}]
["40069","40","OK","069","Johnston","","2104008610","Hydronic heater: outdoor","Hydronic heater",27.30617470592951,"A","CEC Survey",2017,15,"I",63.52520526678761,"TON",8,{"v":2.3264044103912207,"d":"2.33"},{"$f":"VLOOKUP(A32479,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.802575864242384,"d":"1.80"}]
["40071","40","OK","071","Kay","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",294.23662354939995,"A","CEC Survey",2017,15,"I",115.18022513284409,"TON",8,{"v":0.3914544142854,"d":"0.39"},{"$f":"VLOOKUP(A32499,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.303311959,"d":"0.30"}]
["40073","40","OK","073","Kingfisher","","2104009000","Wax Log; Total: All Combustor Types",null,81.73967465733534,"A","CEC Survey",2017,15,"I",19.137898028773634,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A32518,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["40075","40","OK","075","Kiowa","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",140.03118510259998,"A","CEC Survey",2017,15,"I",166.88463474272828,"TON",8,{"v":1.1917676381903999,"d":"1.19"},{"$f":"VLOOKUP(A32535,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.923421384,"d":"0.92"}]
["40079","40","OK","079","Le Flore","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",120.56983989748645,"A","CEC Survey",2017,15,"I",299.79248232518876,"TON",8,{"v":2.4864633027636507,"d":"2.49"},{"$f":"VLOOKUP(A32552,cordwood_density!A:D,4,FALSE)","v":1.3991},{"v":1.7771876940630766,"d":"1.78"}]
["40081","40","OK","081","Lincoln","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",361.07506043550995,"A","CEC Survey",2017,15,"I",175.3204459299492,"TON",8,{"v":0.4855512472074,"d":"0.49"},{"$f":"VLOOKUP(A32574,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.376221329,"d":"0.38"}]
["40087","40","OK","087","Mcclain","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.961175683887975,"A","CEC Survey",2017,15,"I",13.69703948931831,"TON",8,{"v":2.2977077368041736,"d":"2.30"},{"$f":"VLOOKUP(A32613,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.7803407227678396,"d":"1.78"}]
["40087","40","OK","087","Mcclain","","2104008100","Fireplace: general","Fireplace: general",1029.687420454,"A","CEC Survey",2017,15,"I",437.7468310424905,"TON",8,{"v":0.4251259385586,"d":"0.43"},{"$f":"VLOOKUP(A32617,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.329401781,"d":"0.33"}]
["40091","40","OK","091","McIntosh","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",297.92278550099996,"A","CEC Survey",2017,15,"I",88.56073189098089,"TON",8,{"v":0.297260687,"d":"0.30"},{"$f":"VLOOKUP(A32652,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.23032751200991788,"d":"0.23"}]
["40093","40","OK","093","Major","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",122.5179374052,"A","CEC Survey",2017,15,"I",165.60662277946668,"TON",8,{"v":1.3516928727894,"d":"1.35"},{"$f":"VLOOKUP(A32669,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.047336799,"d":"1.05"}]
["40097","40","OK","097","Mayes","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",327.5836508516,"A","CEC Survey",2017,15,"I",188.37434069896813,"TON",8,{"v":0.5750419479398999,"d":"0.58"},{"$f":"VLOOKUP(A32693,cordwood_density!A:D,4,FALSE)","v":1.4581},{"v":0.394377579,"d":"0.39"}]
["40099","40","OK","099","Murray","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",111.36575452950001,"A","CEC Survey",2017,15,"I",54.53433587233352,"TON",8,{"v":0.489686763249,"d":"0.49"},{"$f":"VLOOKUP(A32708,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.379425665,"d":"0.38"}]
["40105","40","OK","105","Nowata","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",18.11412670269653,"A","CEC Survey",2017,15,"I",42.212370719526824,"TON",8,{"v":2.330356379435225,"d":"2.33"},{"$f":"VLOOKUP(A32747,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.8056379818961918,"d":"1.81"}]
["40107","40","OK","107","Okfuskee","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",115.14459369015,"A","CEC Survey",2017,15,"I",62.82885996209216,"TON",8,{"v":0.545651844768,"d":"0.55"},{"$f":"VLOOKUP(A32769,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.42278928,"d":"0.42"}]
["40109","40","OK","109","Oklahoma","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,25348.084748742,"A","CEC Survey",2017,15,"I",9932.59518850847,"TON",8,{"v":0.39184795565279995,"d":"0.39"},{"$f":"VLOOKUP(A32786,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.303616888,"d":"0.30"}]
["40113","40","OK","113","Osage","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",89.75147068195072,"A","CEC Survey",2017,15,"I",208.63611745300335,"TON",8,{"v":2.324598314297714,"d":"2.32"},{"$f":"VLOOKUP(A32807,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.8011764406459896,"d":"1.80"}]
["40115","40","OK","115","Ottawa","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",53.730027117500526,"A","CEC Survey",2017,15,"I",143.25033686417441,"TON",8,{"v":2.666113243362128,"d":"2.67"},{"$f":"VLOOKUP(A32822,cordwood_density!A:D,4,FALSE)","v":1.4903},{"v":1.7889775504006764,"d":"1.79"}]
["40117","40","OK","117","Pawnee","","2104008100","Fireplace: general","Fireplace: general",432.6822716563361,"A","CEC Survey",2017,15,"I",182.42123520820485,"TON",8,{"v":0.421605522477,"d":"0.42"},{"$f":"VLOOKUP(A32842,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.326674045,"d":"0.33"}]
["40119","40","OK","119","Payne","","2104009000","Wax Log; Total: All Combustor Types",null,436.69180605897446,"A","CEC Survey",2017,15,"I",102.24365694374163,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A32863,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["40125","40","OK","125","Pottawatomie","","2104008100","Fireplace: general","Fireplace: general",2691.84091865,"A","CEC Survey",2017,15,"I",1016.948290285095,"TON",8,{"v":0.37778914914300005,"d":"0.38"},{"$f":"VLOOKUP(A32902,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.292723655,"d":"0.29"}]
["40125","40","OK","125","Pottawatomie","","2104009000","Wax Log; Total: All Combustor Types",null,372.3600536797432,"A","CEC Survey",2017,15,"I",87.18151579616173,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A32908,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["40129","40","OK","129","Roger Mills","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",52.38927703800001,"A","CEC Survey",2017,15,"I",69.69435129902224,"TON",8,{"v":1.3303171037933998,"d":"1.33"},{"$f":"VLOOKUP(A32941,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.0307741389999998,"d":"1.03"}]
["40133","40","OK","133","Seminole","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.194104288204373,"A","CEC Survey",2017,15,"I",9.698000473646166,"TON",8,{"v":2.312293592918307,"d":"2.31"},{"$f":"VLOOKUP(A32958,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.7916423314104346,"d":"1.79"}]
["40135","40","OK","135","Sequoyah","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",575.90731001084,"A","CEC Survey",2017,15,"I",886.2780119236278,"TON",8,{"v":1.5389247479893005,"d":"1.54"},{"$f":"VLOOKUP(A32984,cordwood_density!A:D,4,FALSE)","v":1.4791},{"v":1.0404467230000003,"d":"1.04"}]
["40137","40","OK","137","Stephens","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",634.9828396639999,"A","CEC Survey",2017,15,"I",113.22742287731356,"TON",8,{"v":0.178315721,"d":"0.18"},{"$f":"VLOOKUP(A32997,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.1381649783046645,"d":"0.14"}]
["40143","40","OK","143","Tulsa","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",14.912352762967902,"A","CEC Survey",2017,15,"I",21.40435708919498,"TON",8,{"v":1.435344068733995,"d":"1.44"},{"$f":"VLOOKUP(A33036,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.1121525404726444,"d":"1.11"}]
["40145","40","OK","145","Wagoner","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",972.4533596635399,"A","CEC Survey",2017,15,"I",1149.0995201128553,"TON",8,{"v":1.1816500078836,"d":"1.18"},{"$f":"VLOOKUP(A33060,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9155819060000001,"d":"0.92"}]
["40147","40","OK","147","Washington","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",570.78645005136,"A","CEC Survey",2017,15,"I",625.550063607127,"TON",8,{"v":1.0959441373403997,"d":"1.10"},{"$f":"VLOOKUP(A33075,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8491741339999999,"d":"0.85"}]
["40151","40","OK","151","Woods","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.3244451245728353,"A","CEC Survey",2017,15,"I",0.7254976546874213,"TON",8,{"v":2.236118220739523,"d":"2.24"},{"$f":"VLOOKUP(A33096,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.7326191079649178,"d":"1.73"}]
["40153","40","OK","153","Woodward","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",110.27303301177055,"A","CEC Survey",2017,15,"I",43.78209849728315,"TON",8,{"v":0.3970335929058,"d":"0.40"},{"$f":"VLOOKUP(A33113,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.307634893,"d":"0.31"}]
["41001","41","OR","001","Baker","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,973.2811511066121,"A","CEC Survey",2017,15,"I",454.0969620243804,"TON",8,{"v":0.4665629879999999,"d":"0.47"},{"$f":"VLOOKUP(A33131,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.45876399999999995,"d":"0.46"}]
["41007","41","OR","007","Clatsop","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",388.2455703796,"A","CEC Survey",2017,15,"I",519.3221767969422,"TON",8,{"v":1.3376126256615999,"d":"1.34"},{"$f":"VLOOKUP(A33174,cordwood_density!A:D,4,FALSE)","v":1.1548},{"v":1.158306742,"d":"1.16"}]
["41009","41","OR","009","Columbia","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",611.0339797417798,"A","CEC Survey",2017,15,"I",806.7867266853449,"TON",8,{"v":1.3203631114366001,"d":"1.32"},{"$f":"VLOOKUP(A33189,cordwood_density!A:D,4,FALSE)","v":1.0346},{"v":1.2762063710000002,"d":"1.28"}]
["41011","41","OR","011","Coos","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1121.33247927581,"A","CEC Survey",2017,15,"I",2543.9740856828166,"TON",8,{"v":2.2687063227899995,"d":"2.27"},{"$f":"VLOOKUP(A33209,cordwood_density!A:D,4,FALSE)","v":1.0305},{"v":2.2015587799999996,"d":"2.20"}]
["41015","41","OR","015","Curry","","2104008620","Hydronic heater: indoor","Hydronic heater",41.13166972547611,"A","CEC Survey",2017,15,"I",187.62429679305995,"TON",8,{"v":4.561553130357101,"d":"4.56"},{"$f":"VLOOKUP(A33230,cordwood_density!A:D,4,FALSE)","v":1.0562},{"v":4.318834624462319,"d":"4.32"}]
["41017","41","OR","017","Deschutes","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",587.7127985379435,"A","CEC Survey",2017,15,"I",2676.2616599317184,"TON",8,{"v":4.553689602454583,"d":"4.55"},{"$f":"VLOOKUP(A33242,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":4.477570897202147,"d":"4.48"}]
["41019","41","OR","019","Douglas","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1801.6097866424,"A","CEC Survey",2017,15,"I",4291.859816824093,"TON",8,{"v":2.3822360694558,"d":"2.38"},{"$f":"VLOOKUP(A33269,cordwood_density!A:D,4,FALSE)","v":1.0267},{"v":2.320284474,"d":"2.32"}]
["41025","41","OR","025","Harney","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",66.51212660131,"A","CEC Survey",2017,15,"I",40.329270611077504,"TON",8,{"v":0.6063446272409999,"d":"0.61"},{"$f":"VLOOKUP(A33308,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.5962090729999999,"d":"0.60"}]
["41027","41","OR","027","Hood River","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",187.58526225684002,"A","CEC Survey",2017,15,"I",252.77193319627722,"TON",8,{"v":1.347504223707,"d":"1.35"},{"$f":"VLOOKUP(A33325,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.3249795710000003,"d":"1.32"}]
["41031","41","OR","031","Jefferson","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.6233033350976047,"A","CEC Survey",2017,15,"I",12.41016140966289,"TON",8,{"v":4.7307382427435325,"d":"4.73"},{"$f":"VLOOKUP(A33351,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":4.651660022363356,"d":"4.65"}]
["41033","41","OR","033","Josephine","","2104008610","Hydronic heater: outdoor","Hydronic heater",293.56177893914054,"A","CEC Survey",2017,15,"I",1317.8594579504768,"TON",8,{"v":4.489206540145975,"d":"4.49"},{"$f":"VLOOKUP(A33364,cordwood_density!A:D,4,FALSE)","v":1.0444},{"v":4.298359383517786,"d":"4.30"}]
["41035","41","OR","035","Klamath","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",456.68499898896,"A","CEC Survey",2017,15,"I",438.8465041183373,"TON",8,{"v":0.9609391705221,"d":"0.96"},{"$f":"VLOOKUP(A33385,cordwood_density!A:D,4,FALSE)","v":1.0227},{"v":0.9396100230000001,"d":"0.94"}]
["41037","41","OR","037","Lake","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",205.3671166566,"A","CEC Survey",2017,15,"I",498.2526128575133,"TON",8,{"v":2.42615575935,"d":"2.43"},{"$f":"VLOOKUP(A33404,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.38560055,"d":"2.39"}]
["41043","41","OR","043","Linn","","2104008100","Fireplace: general","Fireplace: general",5182.000200065,"A","CEC Survey",2017,15,"I",3061.8774498365,"TON",8,{"v":0.5908678756512,"d":"0.59"},{"$f":"VLOOKUP(A33442,cordwood_density!A:D,4,FALSE)","v":1.0266},{"v":0.575558032,"d":"0.58"}]
["41045","41","OR","045","Malheur","","2104009000","Wax Log; Total: All Combustor Types",null,0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A33463,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["41047","41","OR","047","Marion","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3656.6070479103096,"A","CEC Survey",2017,15,"I",6961.001162656473,"TON",8,{"v":1.9036776638699993,"d":"1.90"},{"$f":"VLOOKUP(A33480,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.8718561099999995,"d":"1.87"}]
["41051","41","OR","051","Multnomah","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",72.10001361185908,"A","CEC Survey",2017,15,"I",24.0844986336612,"TON",8,{"v":0.33404291382407947,"d":"0.33"},{"$f":"VLOOKUP(A33498,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.32845910897156294,"d":"0.33"}]
["41053","41","OR","053","Polk","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",740.77246067528,"A","CEC Survey",2017,15,"I",851.1889839579368,"TON",8,{"v":1.149055923572,"d":"1.15"},{"$f":"VLOOKUP(A33519,cordwood_density!A:D,4,FALSE)","v":1.0424},{"v":1.102317655,"d":"1.10"}]
["41055","41","OR","055","Sherman","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",17.04216084524,"A","CEC Survey",2017,15,"I",9.879542146736712,"TON",8,{"v":0.5797118238968,"d":"0.58"},{"$f":"VLOOKUP(A33533,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.5641415179999999,"d":"0.56"}]
["41059","41","OR","059","Umatilla","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.964810582932296,"A","CEC Survey",2017,15,"I",47.069816560791466,"TON",8,{"v":4.292807085428345,"d":"4.29"},{"$f":"VLOOKUP(A33558,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":4.221049248208796,"d":"4.22"}]
["41063","41","OR","063","Wallowa","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",142.638304656,"A","CEC Survey",2017,15,"I",288.55532191048377,"TON",8,{"v":2.0229862,"d":"2.02"},{"$f":"VLOOKUP(A33597,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9891703048180926,"d":"1.99"}]
["41065","41","OR","065","Wasco","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",271.50462684949997,"A","CEC Survey",2017,15,"I",205.9614741326218,"TON",8,{"v":0.75859287012,"d":"0.76"},{"$f":"VLOOKUP(A33609,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.74591236,"d":"0.75"}]
["41069","41","OR","069","Wheeler","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.34484787750658025,"A","CEC Survey",2017,15,"I",1.662663902952918,"TON",8,{"v":4.82144160194575,"d":"4.82"},{"$f":"VLOOKUP(A33636,cordwood_density!A:D,4,FALSE)","v":1.0262},{"v":4.698344963891786,"d":"4.70"}]
["41071","41","OR","071","Yamhill","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",774.02519588352,"A","CEC Survey",2017,15,"I",869.5293429870688,"TON",8,{"v":1.1233863543608997,"d":"1.12"},{"$f":"VLOOKUP(A33653,cordwood_density!A:D,4,FALSE)","v":1.0269},{"v":1.0939588609999997,"d":"1.09"}]
["42001","42","PA","001","Adams","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",805.97787314304,"A","CEC Survey",2017,15,"I",1161.8804054689163,"TON",8,{"v":1.4415785397904004,"d":"1.44"},{"$f":"VLOOKUP(A33674,cordwood_density!A:D,4,FALSE)","v":1.3904},{"v":1.0368085010000003,"d":"1.04"}]
["42005","42","PA","005","Armstrong","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",303.3689053352726,"A","CEC Survey",2017,15,"I",739.4881021251259,"TON",8,{"v":2.437587007501213,"d":"2.44"},{"$f":"VLOOKUP(A33692,cordwood_density!A:D,4,FALSE)","v":1.2539},{"v":1.9440043125458275,"d":"1.94"}]
["42009","42","PA","009","Bedford","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3250.032932671385,"A","CEC Survey",2017,15,"I",941.492032747267,"TON",8,{"$f":"P33731/J33731","v":{"v":0.28968692079479996,"d":"0.29"}},{"$f":"VLOOKUP(A33731,cordwood_density!A:D,4,FALSE)","v":1.3316},{"$f":"S33731/T33731","v":{"v":0.217548003,"d":"0.22"}}]
["42013","42","PA","013","Blair","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",392.3018070926419,"A","CEC Survey",2017,15,"I",1044.119155459301,"TON",8,{"v":2.661520127060574,"d":"2.66"},{"$f":"VLOOKUP(A33752,cordwood_density!A:D,4,FALSE)","v":1.344},{"v":1.9802977135867363,"d":"1.98"}]
["42015","42","PA","015","Bradford","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.406984924339183,"A","CEC Survey",2017,15,"I",29.003819720841374,"TON",8,{"v":2.7869570227789144,"d":"2.79"},{"$f":"VLOOKUP(A33771,cordwood_density!A:D,4,FALSE)","v":1.2691},{"v":2.1960105766124927,"d":"2.20"}]
["42017","42","PA","017","Bucks","","2104008100","Fireplace: general","Fireplace: general",22745.201857259002,"A","CEC Survey",2017,15,"I",6371.844952595976,"TON",8,{"v":0.28014018044699995,"d":"0.28"},{"$f":"VLOOKUP(A33787,cordwood_density!A:D,4,FALSE)","v":1.3885},{"v":0.20175742199999996,"d":"0.20"}]
["42019","42","PA","019","Butler","","2104009000","Wax Log; Total: All Combustor Types",null,1290.2725080931261,"A","CEC Survey",2017,15,"I",1007.0504670406395,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A33808,cordwood_density!A:D,4,FALSE)","v":1.2584},{"v":0.6202275905912269,"d":"0.62"}]
["42021","42","PA","021","Cambria","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1075.67409955488,"A","CEC Survey",2017,15,"I",1514.0548713425908,"TON",8,{"v":1.4075405106147998,"d":"1.41"},{"$f":"VLOOKUP(A33824,cordwood_density!A:D,4,FALSE)","v":1.3396},{"v":1.0507170129999999,"d":"1.05"}]
["42025","42","PA","025","Carbon","","2104008100","Fireplace: general","Fireplace: general",3215.485712236,"A","CEC Survey",2017,15,"I",1057.37666586167,"TON",8,{"v":0.32883886307999993,"d":"0.33"},{"$f":"VLOOKUP(A33847,cordwood_density!A:D,4,FALSE)","v":1.2264},{"v":0.26813344999999994,"d":"0.27"}]
["42029","42","PA","029","Chester","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",5244.75815639238,"A","CEC Survey",2017,15,"I",5821.968150730171,"TON",8,{"v":1.11005464449,"d":"1.11"},{"$f":"VLOOKUP(A33886,cordwood_density!A:D,4,FALSE)","v":1.389},{"v":0.7991754099999999,"d":"0.80"}]
["42031","42","PA","031","Clarion","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1011.5865680374999,"A","CEC Survey",2017,15,"I",1678.3190351487099,"TON",8,{"v":1.6590958086807,"d":"1.66"},{"$f":"VLOOKUP(A33900,cordwood_density!A:D,4,FALSE)","v":1.3403},{"v":1.237854069,"d":"1.24"}]
["42035","42","PA","035","Clinton","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",474.42328449300004,"A","CEC Survey",2017,15,"I",480.32279569740865,"TON",8,{"v":1.0124351215407001,"d":"1.01"},{"$f":"VLOOKUP(A33925,cordwood_density!A:D,4,FALSE)","v":1.2681},{"v":0.7983874470000001,"d":"0.80"}]
["42037","42","PA","037","Columbia","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",832.32928072,"A","CEC Survey",2017,15,"I",630.0432958246291,"TON",8,{"v":0.756963993,"d":"0.76"},{"$f":"VLOOKUP(A33942,cordwood_density!A:D,4,FALSE)","v":1.2795},{"v":0.5916092168815943,"d":"0.59"}]
["42041","42","PA","041","Cumberland","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",3058.1409704454404,"A","CEC Survey",2017,15,"I",3791.6315581077074,"TON",8,{"v":1.2398485206374998,"d":"1.24"},{"$f":"VLOOKUP(A33976,cordwood_density!A:D,4,FALSE)","v":1.3945},{"v":0.8890989749999998,"d":"0.89"}]
["42043","42","PA","043","Dauphin","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",15.033789311336255,"A","CEC Survey",2017,15,"I",42.01403402498288,"TON",8,{"v":2.794640336837907,"d":"2.79"},{"$f":"VLOOKUP(A33981,cordwood_density!A:D,4,FALSE)","v":1.3796},{"v":2.0256888495490775,"d":"2.03"}]
["42047","42","PA","047","Elk","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",896.0924949270001,"A","CEC Survey",2017,15,"I",1358.2059879473493,"TON",8,{"v":1.5156984302809,"d":"1.52"},{"$f":"VLOOKUP(A34020,cordwood_density!A:D,4,FALSE)","v":1.2479},{"v":1.214599271,"d":"1.21"}]
["42051","42","PA","051","Fayette","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",15.271718246024552,"A","CEC Survey",2017,15,"I",42.24188841847205,"TON",8,{"v":2.7660206754710277,"d":"2.77"},{"$f":"VLOOKUP(A34041,cordwood_density!A:D,4,FALSE)","v":1.3531},{"v":2.0442100919895263,"d":"2.04"}]
["42053","42","PA","053","Forest","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",62.657673424500004,"A","CEC Survey",2017,15,"I",57.67781122462405,"TON",8,{"v":0.9205227081105,"d":"0.92"},{"$f":"VLOOKUP(A34059,cordwood_density!A:D,4,FALSE)","v":1.2399},{"v":0.742416895,"d":"0.74"}]
["42055","42","PA","055","Franklin","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,8072.220105053999,"A","CEC Survey",2017,15,"I",2374.9359389964075,"TON",8,{"v":0.2942109987201,"d":"0.29"},{"$f":"VLOOKUP(A34076,cordwood_density!A:D,4,FALSE)","v":1.3797},{"v":0.213242733,"d":"0.21"}]
["42057","42","PA","057","Fulton","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",227.94808946648996,"A","CEC Survey",2017,15,"I",399.9508404059026,"TON",8,{"v":1.7545698292185,"d":"1.75"},{"$f":"VLOOKUP(A34094,cordwood_density!A:D,4,FALSE)","v":1.3405},{"v":1.3088920769999999,"d":"1.31"}]
["42061","42","PA","061","Huntingdon","","2104008620","Hydronic heater: indoor","Hydronic heater",178.62304333991273,"A","CEC Survey",2017,15,"I",537.5315627286119,"TON",8,{"$f":"P34115/J34115","v":{"v":3.009306933068597,"d":"3.01"}},{"$f":"VLOOKUP(A34115,cordwood_density!A:D,4,FALSE)","v":1.3654},{"$f":"S34115/T34115","v":{"v":2.203974610420827,"d":"2.20"}}]
["42063","42","PA","063","Indiana","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4838.49895811,"A","CEC Survey",2017,15,"I",1317.8425369541,"TON",8,{"v":0.27236598547679997,"d":"0.27"},{"$f":"VLOOKUP(A34136,cordwood_density!A:D,4,FALSE)","v":1.2634},{"v":0.21558175199999996,"d":"0.22"}]
["42069","42","PA","069","Lackawanna","","2104008620","Hydronic heater: indoor","Hydronic heater",401.29127956298737,"A","CEC Survey",2017,15,"I",978.0852280193955,"TON",8,{"v":2.43734483611143,"d":"2.44"},{"$f":"VLOOKUP(A34175,cordwood_density!A:D,4,FALSE)","v":1.2781},{"v":1.9070063657862686,"d":"1.91"}]
["42071","42","PA","071","Lancaster","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",21.08149060059119,"A","CEC Survey",2017,15,"I",55.49931940048899,"TON",8,{"v":2.6326088819797504,"d":"2.63"},{"$f":"VLOOKUP(A34191,cordwood_density!A:D,4,FALSE)","v":1.3909},{"v":1.8927377108201526,"d":"1.89"}]
["42073","42","PA","073","Lawrence","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",621.2692728624,"A","CEC Survey",2017,15,"I",798.2724182301703,"TON",8,{"v":1.2849056811586,"d":"1.28"},{"$f":"VLOOKUP(A34214,cordwood_density!A:D,4,FALSE)","v":1.2598},{"v":1.0199283069999998,"d":"1.02"}]
["42075","42","PA","075","Lebanon","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1708.1058428497602,"A","CEC Survey",2017,15,"I",2160.84608877724,"TON",8,{"v":1.2650539764983997,"d":"1.27"},{"$f":"VLOOKUP(A34231,cordwood_density!A:D,4,FALSE)","v":1.3992},{"v":0.9041266269999998,"d":"0.90"}]
["42081","42","PA","081","Lycoming","","2104008100","Fireplace: general","Fireplace: general",6854.76975843546,"A","CEC Survey",2017,15,"I",2301.8986942272986,"TON",8,{"v":0.33580977557919994,"d":"0.34"},{"$f":"VLOOKUP(A34267,cordwood_density!A:D,4,FALSE)","v":1.3247},{"v":0.25349873599999995,"d":"0.25"}]
["42081","42","PA","081","Lycoming","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1126.2476952740446,"A","CEC Survey",2017,15,"I",1069.0310556418897,"TON",8,{"v":0.9491971083516999,"d":"0.95"},{"$f":"VLOOKUP(A34270,cordwood_density!A:D,4,FALSE)","v":1.3247},{"v":0.7165374109999999,"d":"0.72"}]
["42087","42","PA","087","Mifflin","","2104008610","Hydronic heater: outdoor","Hydronic heater",223.68155415451267,"A","CEC Survey",2017,15,"I",658.7801857549688,"TON",8,{"v":2.9451699235776174,"d":"2.95"},{"$f":"VLOOKUP(A34309,cordwood_density!A:D,4,FALSE)","v":1.3568},{"v":2.1706735875424656,"d":"2.17"}]
["42089","42","PA","089","Monroe","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2127.493377212,"A","CEC Survey",2017,15,"I",2968.979332817831,"TON",8,{"v":1.395529295,"d":"1.40"},{"$f":"VLOOKUP(A34332,cordwood_density!A:D,4,FALSE)","v":1.257},{"v":1.110206280827367,"d":"1.11"}]
["42091","42","PA","091","Montgomery","","2104009000","Wax Log; Total: All Combustor Types",null,7918.220985015926,"A","CEC Survey",2017,15,"I",1108.5509379022299,"TON",8,0.14,{"$f":"VLOOKUP(A34348,cordwood_density!A:D,4,FALSE)","v":1.3886},{"v":0.10082097076191848,"d":"0.10"}]
["42093","42","PA","093","Montour","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",497.5530713985,"A","CEC Survey",2017,15,"I",697.9025376854065,"TON",8,{"v":1.4026695398015998,"d":"1.40"},{"$f":"VLOOKUP(A34365,cordwood_density!A:D,4,FALSE)","v":1.3272},{"v":1.056863728,"d":"1.06"}]
["42097","42","PA","097","Northumberland","","2104008620","Hydronic heater: indoor","Hydronic heater",185.56613617102687,"A","CEC Survey",2017,15,"I",529.3336507412514,"TON",8,{"v":2.8525336662363414,"d":"2.85"},{"$f":"VLOOKUP(A34385,cordwood_density!A:D,4,FALSE)","v":1.3247},{"v":2.1533431465511748,"d":"2.15"}]
["42099","42","PA","099","Perry","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",896.951980696,"A","CEC Survey",2017,15,"I",780.0182014850571,"TON",8,{"v":0.8696320631119999,"d":"0.87"},{"$f":"VLOOKUP(A34404,cordwood_density!A:D,4,FALSE)","v":1.3697},{"v":0.63490696,"d":"0.63"}]
["42105","42","PA","105","Potter","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.725465566415492,"A","CEC Survey",2017,15,"I",27.269249450565702,"TON",8,{"v":2.542476993814939,"d":"2.54"},{"$f":"VLOOKUP(A34443,cordwood_density!A:D,4,FALSE)","v":1.2061},{"v":2.108015084831224,"d":"2.11"}]
["42107","42","PA","107","Schuylkill","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",15.285128829738293,"A","CEC Survey",2017,15,"I",44.602613738050195,"TON",8,{"v":2.9180397649820704,"d":"2.92"},{"$f":"VLOOKUP(A34461,cordwood_density!A:D,4,FALSE)","v":1.2835},{"v":2.2735019594718118,"d":"2.27"}]
["42109","42","PA","109","Snyder","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",560.093732,"A","CEC Survey",2017,15,"I",485.3731501087374,"TON",8,{"v":0.866592719,"d":"0.87"},{"$f":"VLOOKUP(A34482,cordwood_density!A:D,4,FALSE)","v":1.3679},{"v":0.6335205197748374,"d":"0.63"}]
["42113","42","PA","113","Sullivan","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.041699792646595,"A","CEC Survey",2017,15,"I",17.725707349384205,"TON",8,{"v":2.9338940956580326,"d":"2.93"},{"$f":"VLOOKUP(A34503,cordwood_density!A:D,4,FALSE)","v":1.2403},{"v":2.365471334078878,"d":"2.37"}]
["42115","42","PA","115","Susquehanna","","2104008620","Hydronic heater: indoor","Hydronic heater",238.99920364961068,"A","CEC Survey",2017,15,"I",677.892414073064,"TON",8,{"v":2.836379384204564,"d":"2.84"},{"$f":"VLOOKUP(A34520,cordwood_density!A:D,4,FALSE)","v":1.2408},{"v":2.285927936979823,"d":"2.29"}]
["42119","42","PA","119","Union","","2104009000","Wax Log; Total: All Combustor Types",null,160.32486192581854,"A","CEC Survey",2017,15,"I",125.13265691387457,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A34558,cordwood_density!A:D,4,FALSE)","v":1.3661},{"v":0.571330356489276,"d":"0.57"}]
["42119","42","PA","119","Union","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",373.07913756928,"A","CEC Survey",2017,15,"I",562.3370697250166,"TON",8,{"v":1.5072862915595,"d":"1.51"},{"$f":"VLOOKUP(A34559,cordwood_density!A:D,4,FALSE)","v":1.3661},{"v":1.103349895,"d":"1.10"}]
["42125","42","PA","125","Washington","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",673.52700871632,"A","CEC Survey",2017,15,"I",445.71398945587435,"TON",8,{"v":0.6617611226985001,"d":"0.66"},{"$f":"VLOOKUP(A34598,cordwood_density!A:D,4,FALSE)","v":1.2639},{"v":0.523586615,"d":"0.52"}]
["42129","42","PA","129","Westmoreland","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",91.92815272606866,"A","CEC Survey",2017,15,"I",223.21496854981743,"TON",8,{"v":2.4281459153754854,"d":"2.43"},{"$f":"VLOOKUP(A34623,cordwood_density!A:D,4,FALSE)","v":1.2641},{"v":1.9208495493833442,"d":"1.92"}]
["42131","42","PA","131","Wyoming","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",241.9437122778692,"A","CEC Survey",2017,15,"I",697.2171944190588,"TON",8,{"v":2.881733060367008,"d":"2.88"},{"$f":"VLOOKUP(A34637,cordwood_density!A:D,4,FALSE)","v":1.2659},{"v":2.276430255444354,"d":"2.28"}]
["42133","42","PA","133","York","","2104008610","Hydronic heater: outdoor","Hydronic heater",785.0410862786682,"A","CEC Survey",2017,15,"I",2090.0237089769385,"TON",8,{"v":2.662311241420856,"d":"2.66"},{"$f":"VLOOKUP(A34654,cordwood_density!A:D,4,FALSE)","v":1.4009},{"v":1.9004291822548762,"d":"1.90"}]
["44001","44","RI","001","Bristol","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,101.404411272,"A","CEC Survey",2017,15,"I",621.8129408356589,"TON",8,{"v":6.132010758070001,"d":"6.13"},{"$f":"VLOOKUP(A34676,cordwood_density!A:D,4,FALSE)","v":1.2934},{"v":4.74100105,"d":"4.74"}]
["44003","44","RI","003","Kent","","2104009000","Wax Log; Total: All Combustor Types",null,1453.493874632905,"A","CEC Survey",2017,15,"I",1134.4438295852844,"TON",8,{"v":0.7804944,"d":"0.78"},{"$f":"VLOOKUP(A34693,cordwood_density!A:D,4,FALSE)","v":1.4877},{"v":0.5246315789473684,"d":"0.52"}]
["44009","44","RI","009","Washington","","2104008100","Fireplace: general","Fireplace: general",4196.828515464,"A","CEC Survey",2017,15,"I",1592.31882405306,"TON",8,{"v":0.37941002787839995,"d":"0.38"},{"$f":"VLOOKUP(A34732,cordwood_density!A:D,4,FALSE)","v":1.4848},{"v":0.255529383,"d":"0.26"}]
["45001","45","SC","001","Abbeville","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",340.78824100799994,"A","CEC Survey",2017,15,"I",52.85210060852994,"TON",8,{"v":0.155087806,"d":"0.16"},{"$f":"VLOOKUP(A34752,cordwood_density!A:D,4,FALSE)","v":1.2454},{"v":0.12452850971575397,"d":"0.12"}]
["45003","45","SC","003","Aiken","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1616.4876135835498,"A","CEC Survey",2017,15,"I",872.6755972049266,"TON",8,{"v":0.5398591302969,"d":"0.54"},{"$f":"VLOOKUP(A34771,cordwood_density!A:D,4,FALSE)","v":1.2751},{"v":0.42338571900000005,"d":"0.42"}]
["45007","45","SC","007","Anderson","","2104008100","Fireplace: general","Fireplace: general",7385.9002914640005,"A","CEC Survey",2017,15,"I",1214.7154255978337,"TON",8,{"v":0.1644640974915,"d":"0.16"},{"$f":"VLOOKUP(A34792,cordwood_density!A:D,4,FALSE)","v":1.3765},{"v":0.11947991100000001,"d":"0.12"}]
["45009","45","SC","009","Bamberg","","2104008620","Hydronic heater: indoor","Hydronic heater",12.834948962830403,"A","CEC Survey",2017,15,"I",13.035116546249156,"TON",8,{"v":1.015595510663769,"d":"1.02"},{"$f":"VLOOKUP(A34805,cordwood_density!A:D,4,FALSE)","v":1.2686},{"v":0.8005640159733322,"d":"0.80"}]
["45011","45","SC","011","Barnwell","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",262.89178982,"A","CEC Survey",2017,15,"I",38.37324564200799,"TON",8,{"v":0.145965934,"d":"0.15"},{"$f":"VLOOKUP(A34827,cordwood_density!A:D,4,FALSE)","v":1.3746},{"v":0.10618793394442018,"d":"0.11"}]
["45017","45","SC","017","Calhoun","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",171.08924973000003,"A","CEC Survey",2017,15,"I",50.06878722742466,"TON",8,{"v":0.29264718447499993,"d":"0.29"},{"$f":"VLOOKUP(A34870,cordwood_density!A:D,4,FALSE)","v":1.1945},{"v":0.24499554999999998,"d":"0.24"}]
["45019","45","SC","019","Charleston","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",6.133812878063629,"A","CEC Survey",2017,15,"I",5.9882300862130515,"TON",8,{"v":0.9762655309601593,"d":"0.98"},{"$f":"VLOOKUP(A34881,cordwood_density!A:D,4,FALSE)","v":1.3289},{"v":0.7346418323125588,"d":"0.73"}]
["45023","45","SC","023","Chester","","2104008610","Hydronic heater: outdoor","Hydronic heater",72.71649807121806,"A","CEC Survey",2017,15,"I",71.9342031745002,"TON",8,{"v":0.9892418513340441,"d":"0.99"},{"$f":"VLOOKUP(A34909,cordwood_density!A:D,4,FALSE)","v":1.27},{"v":0.7789305916016095,"d":"0.78"}]
["45025","45","SC","025","Chesterfield","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.2251815974447497,"A","CEC Survey",2017,15,"I",2.172300832149904,"TON",8,{"v":0.9762353035116008,"d":"0.98"},{"$f":"VLOOKUP(A34926,cordwood_density!A:D,4,FALSE)","v":1.1987},{"v":0.814411698933512,"d":"0.81"}]
["45027","45","SC","027","Clarendon","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",395.68515913619,"A","CEC Survey",2017,15,"I",106.01127833677023,"TON",8,{"v":0.26791825745549996,"d":"0.27"},{"$f":"VLOOKUP(A34943,cordwood_density!A:D,4,FALSE)","v":1.2549},{"v":0.213497695,"d":"0.21"}]
["45031","45","SC","031","Darlington","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",101.70641753036256,"A","CEC Survey",2017,15,"I",109.03825250525138,"TON",8,{"v":1.0720882236629763,"d":"1.07"},{"$f":"VLOOKUP(A34967,cordwood_density!A:D,4,FALSE)","v":1.3313},{"v":0.8052942414654671,"d":"0.81"}]
["45035","45","SC","035","Dorchester","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1894.6405396339198,"A","CEC Survey",2017,15,"I",752.8721425673749,"TON",8,{"v":0.3973693831722,"d":"0.40"},{"$f":"VLOOKUP(A35004,cordwood_density!A:D,4,FALSE)","v":1.2891},{"v":0.30825334200000004,"d":"0.31"}]
["45037","45","SC","037","Edgefield","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1355.76646731,"A","CEC Survey",2017,15,"I",167.93865181493183,"TON",8,{"v":0.1238698963754,"d":"0.12"},{"$f":"VLOOKUP(A35021,cordwood_density!A:D,4,FALSE)","v":1.2761},{"v":0.097069114,"d":"0.10"}]
["45041","45","SC","041","Florence","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.98975474567349,"A","CEC Survey",2017,15,"I",14.324611824147881,"TON",8,{"v":1.0239358791173911,"d":"1.02"},{"$f":"VLOOKUP(A35043,cordwood_density!A:D,4,FALSE)","v":1.291},{"v":0.7931339110126965,"d":"0.79"}]
["45043","45","SC","043","Georgetown","","2104008620","Hydronic heater: indoor","Hydronic heater",47.20346670310955,"A","CEC Survey",2017,15,"I",51.26052866735563,"TON",8,{"v":1.085948389972358,"d":"1.09"},{"$f":"VLOOKUP(A35060,cordwood_density!A:D,4,FALSE)","v":1.3384},{"v":0.8113780558669741,"d":"0.81"}]
["45045","45","SC","045","Greenville","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,22775.637102568,"A","CEC Survey",2017,15,"I",3144.0914262161136,"TON",8,{"v":0.1380462558328,"d":"0.14"},{"$f":"VLOOKUP(A35081,cordwood_density!A:D,4,FALSE)","v":1.3496},{"v":0.10228679300000001,"d":"0.10"}]
["45047","45","SC","047","Greenwood","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3719.3525568355835,"A","CEC Survey",2017,15,"I",459.77370537353374,"TON",8,{"v":0.1236165967995,"d":"0.12"},{"$f":"VLOOKUP(A35096,cordwood_density!A:D,4,FALSE)","v":1.2855},{"v":0.096162269,"d":"0.10"}]
["45053","45","SC","053","Jasper","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",272.78214728755,"A","CEC Survey",2017,15,"I",89.04582144960811,"TON",8,{"v":0.32643566426559995,"d":"0.33"},{"$f":"VLOOKUP(A35138,cordwood_density!A:D,4,FALSE)","v":1.2832},{"v":0.254391883,"d":"0.25"}]
["45055","45","SC","055","Kershaw","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",939.22993932792,"A","CEC Survey",2017,15,"I",558.2574317792905,"TON",8,{"v":0.5943778071840001,"d":"0.59"},{"$f":"VLOOKUP(A35159,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.4670578400000001,"d":"0.47"}]
["45057","45","SC","057","Lancaster","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1103.167608805,"A","CEC Survey",2017,15,"I",152.27448547665938,"TON",8,{"v":0.138033862,"d":"0.14"},{"$f":"VLOOKUP(A35172,cordwood_density!A:D,4,FALSE)","v":1.2187},{"v":0.11326320013128745,"d":"0.11"}]
["45061","45","SC","061","Lee","","2104008610","Hydronic heater: outdoor","Hydronic heater",27.235597778552993,"A","CEC Survey",2017,15,"I",30.148115311611807,"TON",8,{"v":1.1069378963788454,"d":"1.11"},{"$f":"VLOOKUP(A35194,cordwood_density!A:D,4,FALSE)","v":1.3443},{"v":0.8234307047376668,"d":"0.82"}]
["45063","45","SC","063","Lexington","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",2294.46053737488,"A","CEC Survey",2017,15,"I",649.727610147773,"TON",8,{"v":0.28317227494839997,"d":"0.28"},{"$f":"VLOOKUP(A35215,cordwood_density!A:D,4,FALSE)","v":1.2751},{"v":0.222078484,"d":"0.22"}]
["45067","45","SC","067","Marion","","2104009000","Wax Log; Total: All Combustor Types",null,171.0773615961204,"A","CEC Survey",2017,15,"I",58.75288444625363,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A35248,cordwood_density!A:D,4,FALSE)","v":1.2448},{"v":0.27589070533419024,"d":"0.28"}]
["45069","45","SC","069","Marlboro","","2104008610","Hydronic heater: outdoor","Hydronic heater",38.479862393395365,"A","CEC Survey",2017,15,"I",38.673029312622816,"TON",8,{"v":1.005019948284966,"d":"1.01"},{"$f":"VLOOKUP(A35254,cordwood_density!A:D,4,FALSE)","v":1.2565},{"v":0.7998567037683773,"d":"0.80"}]
["45073","45","SC","073","Oconee","","2104009000","Wax Log; Total: All Combustor Types",null,450.33662962679534,"A","CEC Survey",2017,15,"I",154.65854579194328,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A35293,cordwood_density!A:D,4,FALSE)","v":1.3704},{"v":0.25060475043782837,"d":"0.25"}]
["45075","45","SC","075","Orangeburg","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.559736634140143,"A","CEC Survey",2017,15,"I",3.5553416960863826,"TON",8,{"v":0.9987653755023307,"d":"1.00"},{"$f":"VLOOKUP(A35301,cordwood_density!A:D,4,FALSE)","v":1.2362},{"v":0.8079318682270916,"d":"0.81"}]
["45079","45","SC","079","Richland","","2104008100","Fireplace: general","Fireplace: general",17311.34523732,"A","CEC Survey",2017,15,"I",2152.7868324684455,"TON",8,{"v":0.12435699265170001,"d":"0.12"},{"$f":"VLOOKUP(A35332,cordwood_density!A:D,4,FALSE)","v":1.2723},{"v":0.09774187900000002,"d":"0.10"}]
["45081","45","SC","081","Saluda","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",285.9168666166,"A","CEC Survey",2017,15,"I",90.91327373666671,"TON",8,{"v":0.3179710060917001,"d":"0.32"},{"$f":"VLOOKUP(A35349,cordwood_density!A:D,4,FALSE)","v":1.2477},{"v":0.2548457210000001,"d":"0.25"}]
["45083","45","SC","083","Spartanburg","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",4199.2956558633605,"A","CEC Survey",2017,15,"I",2207.5626068619836,"TON",8,{"v":0.5256983046144,"d":"0.53"},{"$f":"VLOOKUP(A35370,cordwood_density!A:D,4,FALSE)","v":1.3092},{"v":0.40154163200000004,"d":"0.40"}]
["45087","45","SC","087","Union","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",67.93772178362269,"A","CEC Survey",2017,15,"I",71.37783907399033,"TON",8,{"v":1.0506363357506188,"d":"1.05"},{"$f":"VLOOKUP(A35387,cordwood_density!A:D,4,FALSE)","v":1.3036},{"v":0.8059499353717542,"d":"0.81"}]
["45091","45","SC","091","York","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2492.0719505988436,"A","CEC Survey",2017,15,"I",333.37383003799766,"TON",8,{"v":0.133773758,"d":"0.13"},{"$f":"VLOOKUP(A35427,cordwood_density!A:D,4,FALSE)","v":1.2239},{"v":0.1093012157856034,"d":"0.11"}]
["46005","46","SD","005","Beadle","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.612911092516542,"A","CEC Survey",2017,15,"I",10.13234484880827,"TON",8,{"v":1.532206422716687,"d":"1.53"},{"$f":"VLOOKUP(A35448,cordwood_density!A:D,4,FALSE)","v":0.9669},{"v":1.5846586231427107,"d":"1.58"}]
["46007","46","SD","007","Bennett","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.642647165816255,"A","CEC Survey",2017,15,"I",3.4862578535265407,"TON",8,{"v":2.122341258717096,"d":"2.12"},{"$f":"VLOOKUP(A35463,cordwood_density!A:D,4,FALSE)","v":1.348},{"v":1.5744371355468068,"d":"1.57"}]
["46009","46","SD","009","Bon Homme","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",20.462242629120002,"A","CEC Survey",2017,15,"I",5.275536603138632,"TON",8,{"v":0.25781810424,"d":"0.26"},{"$f":"VLOOKUP(A35483,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":0.207917826,"d":"0.21"}]
["46011","46","SD","011","Brookings","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",170.74857751944,"A","CEC Survey",2017,15,"I",153.71761888367405,"TON",8,{"v":0.9002570979905999,"d":"0.90"},{"$f":"VLOOKUP(A35504,cordwood_density!A:D,4,FALSE)","v":1.2379},{"v":0.727245414,"d":"0.73"}]
["46017","46","SD","017","Buffalo","","2104008610","Hydronic heater: outdoor","Hydronic heater",12.516201444483514,"A","CEC Survey",2017,15,"I",18.526410867329577,"TON",8,{"v":1.4801943664381536,"d":"1.48"},{"$f":"VLOOKUP(A35539,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":1.6019419550196468,"d":"1.60"}]
["46017","46","SD","017","Buffalo","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",4.415832397199999,"A","CEC Survey",2017,15,"I",0.796306796430151,"TON",8,{"v":0.180329941176,"d":"0.18"},{"$f":"VLOOKUP(A35543,cordwood_density!A:D,4,FALSE)","v":0.924},{"v":0.195162274,"d":"0.20"}]
["46023","46","SD","023","Charles Mix","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",76.13985942482628,"A","CEC Survey",2017,15,"I",150.10099050308398,"TON",8,{"v":1.971385180337512,"d":"1.97"},{"$f":"VLOOKUP(A35582,cordwood_density!A:D,4,FALSE)","v":1.2398},{"v":1.5900832233727311,"d":"1.59"}]
["46023","46","SD","023","Charles Mix","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",158.116478432,"A","CEC Survey",2017,15,"I",95.42611995894862,"TON",8,{"v":0.603517868,"d":"0.60"},{"$f":"VLOOKUP(A35592,cordwood_density!A:D,4,FALSE)","v":1.2398},{"v":0.48678647201161473,"d":"0.49"}]
["46027","46","SD","027","Clay","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,547.90942228,"A","CEC Survey",2017,15,"I",103.78032806048034,"TON",8,{"v":0.18941146810110002,"d":"0.19"},{"$f":"VLOOKUP(A35621,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.153134019,"d":"0.15"}]
["46029","46","SD","029","Codington","","2104009000","Wax Log; Total: All Combustor Types",null,192.6783043515331,"A","CEC Survey",2017,15,"I",150.38433754786718,"TON",8,{"v":0.7804943999999998,"d":"0.78"},{"$f":"VLOOKUP(A35638,cordwood_density!A:D,4,FALSE)","v":1.1183},{"v":0.6979293570598227,"d":"0.70"}]
["46033","46","SD","033","Custer","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",101.49248582108076,"A","CEC Survey",2017,15,"I",216.12667213178034,"TON",8,{"v":2.129484467577098,"d":"2.13"},{"$f":"VLOOKUP(A35657,cordwood_density!A:D,4,FALSE)","v":1.294},{"v":1.645660330430524,"d":"1.65"}]
["46035","46","SD","035","Davison","","2104008100","Fireplace: general","Fireplace: general",594.7298316516088,"A","CEC Survey",2017,15,"I",137.51841654399573,"TON",8,{"v":0.23122838173779997,"d":"0.23"},{"$f":"VLOOKUP(A35677,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.19233769899999997,"d":"0.19"}]
["46039","46","SD","039","Deuel","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",141.21357867929436,"A","CEC Survey",2017,15,"I",137.27550110664345,"TON",8,{"v":0.9721126140312997,"d":"0.97"},{"$f":"VLOOKUP(A35716,cordwood_density!A:D,4,FALSE)","v":1.1299},{"v":0.8603527869999997,"d":"0.86"}]
["46043","46","SD","043","Douglas","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.459463603083917,"A","CEC Survey",2017,15,"I",4.546248211980122,"TON",8,{"v":1.8484714334782548,"d":"1.85"},{"$f":"VLOOKUP(A35733,cordwood_density!A:D,4,FALSE)","v":1.1577},{"v":1.596675678913583,"d":"1.60"}]
["46045","46","SD","045","Edmunds","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",32.58660215755,"A","CEC Survey",2017,15,"I",7.397208442056047,"TON",8,{"v":0.2270015267714,"d":"0.23"},{"$f":"VLOOKUP(A35755,cordwood_density!A:D,4,FALSE)","v":1.1299},{"v":0.20090408600000004,"d":"0.20"}]
["46047","46","SD","047","Fall River","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",102.23694152,"A","CEC Survey",2017,15,"I",55.778335576362934,"TON",8,{"v":0.545579071,"d":"0.55"},{"$f":"VLOOKUP(A35772,cordwood_density!A:D,4,FALSE)","v":1.0926},{"v":0.499340171151382,"d":"0.50"}]
["46051","46","SD","051","Grant","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.540606850898803,"A","CEC Survey",2017,15,"I",9.482454572470521,"TON",8,{"v":2.0883672345676634,"d":"2.09"},{"$f":"VLOOKUP(A35793,cordwood_density!A:D,4,FALSE)","v":1.2873},{"v":1.6222848089549158,"d":"1.62"}]
["46055","46","SD","055","Haakon","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",22.191143765,"A","CEC Survey",2017,15,"I",5.580839202084001,"TON",8,{"v":0.2514894798206,"d":"0.25"},{"$f":"VLOOKUP(A35830,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.19336420099999999,"d":"0.19"}]
["46055","46","SD","055","Haakon","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",41.104137216999995,"A","CEC Survey",2017,15,"I",22.18846977228453,"TON",8,{"v":0.539811106,"d":"0.54"},{"$f":"VLOOKUP(A35832,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.41504775180685843,"d":"0.42"}]
["46061","46","SD","061","Hanson","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.6945019565501106,"A","CEC Survey",2017,15,"I",1.3151059939864846,"TON",8,{"v":1.8935958085981222,"d":"1.89"},{"$f":"VLOOKUP(A35871,cordwood_density!A:D,4,FALSE)","v":1.1942},{"v":1.5856605330749642,"d":"1.59"}]
["46063","46","SD","063","Harding","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.0741496951641405,"A","CEC Survey",2017,15,"I",2.304572394006872,"TON",8,{"v":2.145485312133064,"d":"2.15"},{"$f":"VLOOKUP(A35883,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.64961195766036,"d":"1.65"}]
["46065","46","SD","065","Hughes","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",410.07306415627,"A","CEC Survey",2017,15,"I",331.35728059046767,"TON",8,{"v":0.8080444914670001,"d":"0.81"},{"$f":"VLOOKUP(A35910,cordwood_density!A:D,4,FALSE)","v":1.151},{"v":0.702036917,"d":"0.70"}]
["46069","46","SD","069","Hyde","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",14.601889527062148,"A","CEC Survey",2017,15,"I",29.029054408839706,"TON",8,{"v":1.9880341071639551,"d":"1.99"},{"$f":"VLOOKUP(A35927,cordwood_density!A:D,4,FALSE)","v":1.24},{"v":1.603253312228996,"d":"1.60"}]
["46073","46","SD","073","Jerauld","","2104008610","Hydronic heater: outdoor","Hydronic heater",26.52327107136484,"A","CEC Survey",2017,15,"I",49.17326603642805,"TON",8,{"v":1.8539668770160365,"d":"1.85"},{"$f":"VLOOKUP(A35959,cordwood_density!A:D,4,FALSE)","v":1.1299},{"v":1.6408238578777208,"d":"1.64"}]
["46073","46","SD","073","Jerauld","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,145.436493879,"A","CEC Survey",2017,15,"I",25.48866374946995,"TON",8,{"v":0.1752563133891,"d":"0.18"},{"$f":"VLOOKUP(A35966,cordwood_density!A:D,4,FALSE)","v":1.1299},{"v":0.155107809,"d":"0.16"}]
["46079","46","SD","079","Lake","","2104008620","Hydronic heater: indoor","Hydronic heater",41.066775903677,"A","CEC Survey",2017,15,"I",74.09698385139005,"TON",8,{"v":1.8043048722691577,"d":"1.80"},{"$f":"VLOOKUP(A36005,cordwood_density!A:D,4,FALSE)","v":1.1299},{"v":1.5968712915029275,"d":"1.60"}]
["46081","46","SD","081","Lawrence","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",274.38275833224003,"A","CEC Survey",2017,15,"I",88.07699768438228,"TON",8,{"v":0.3210004820264,"d":"0.32"},{"$f":"VLOOKUP(A36024,cordwood_density!A:D,4,FALSE)","v":1.0274},{"v":0.312439636,"d":"0.31"}]
["46083","46","SD","083","Lincoln","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",224.14850172671999,"A","CEC Survey",2017,15,"I",188.08896834789138,"TON",8,{"v":0.8391265919645,"d":"0.84"},{"$f":"VLOOKUP(A36044,cordwood_density!A:D,4,FALSE)","v":1.2145},{"v":0.6909235010000001,"d":"0.69"}]
["46085","46","SD","085","Lyman","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",122.12892695744999,"A","CEC Survey",2017,15,"I",129.24390437024567,"TON",8,{"v":1.0582579212807999,"d":"1.06"},{"$f":"VLOOKUP(A36061,cordwood_density!A:D,4,FALSE)","v":1.2322},{"v":0.858836164,"d":"0.86"}]
["46089","46","SD","089","McPherson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",32.99102555213134,"A","CEC Survey",2017,15,"I",61.27341138011518,"TON",8,{"v":1.857275133302326,"d":"1.86"},{"$f":"VLOOKUP(A36077,cordwood_density!A:D,4,FALSE)","v":1.1299},{"v":1.6437517774159893,"d":"1.64"}]
["46091","46","SD","091","Marshall","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",43.448083319549994,"A","CEC Survey",2017,15,"I",11.422543541999424,"TON",8,{"v":0.26290097673560003,"d":"0.26"},{"$f":"VLOOKUP(A36100,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.20213822600000003,"d":"0.20"}]
["46093","46","SD","093","Meade","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",497.5471275389999,"A","CEC Survey",2017,15,"I",448.4391787441198,"TON",8,{"v":0.9012999049200001,"d":"0.90"},{"$f":"VLOOKUP(A36121,cordwood_density!A:D,4,FALSE)","v":1.1826},{"v":0.7621342,"d":"0.76"}]
["46099","46","SD","099","Minnehaha","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",33.835336375854126,"A","CEC Survey",2017,15,"I",59.01547627669925,"TON",8,{"v":1.744196529366098,"d":"1.74"},{"$f":"VLOOKUP(A36153,cordwood_density!A:D,4,FALSE)","v":1.1768},{"v":1.4821520473879146,"d":"1.48"}]
["46101","46","SD","101","Moody","","2104009000","Wax Log; Total: All Combustor Types",null,42.73540942467787,"A","CEC Survey",2017,15,"I",33.3547477376683,"TON",8,{"v":0.7804944,"d":"0.78"},{"$f":"VLOOKUP(A36178,cordwood_density!A:D,4,FALSE)","v":1.2168},{"v":0.6414319526627219,"d":"0.64"}]
["46103","46","SD","103","Pennington","","2104008610","Hydronic heater: outdoor","Hydronic heater",276.14448911310063,"A","CEC Survey",2017,15,"I",439.0956580262197,"TON",8,{"v":1.5900938651228311,"d":"1.59"},{"$f":"VLOOKUP(A36199,cordwood_density!A:D,4,FALSE)","v":1.0576},{"v":1.5034926863869431,"d":"1.50"}]
["46105","46","SD","105","Perkins","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9435277838207599,"A","CEC Survey",2017,15,"I",1.591300082221794,"TON",8,{"v":1.6865428973145005,"d":"1.69"},{"$f":"VLOOKUP(A36216,cordwood_density!A:D,4,FALSE)","v":1.031},{"v":1.6358321021479152,"d":"1.64"}]
["46109","46","SD","109","Roberts","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",94.57413814799999,"A","CEC Survey",2017,15,"I",22.584338946400187,"TON",8,{"v":0.238800367507,"d":"0.24"},{"$f":"VLOOKUP(A36250,cordwood_density!A:D,4,FALSE)","v":1.1765},{"v":0.202975238,"d":"0.20"}]
["46109","46","SD","109","Roberts","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",544.3489158457201,"A","CEC Survey",2017,15,"I",564.4732833228304,"TON",8,{"v":1.0369696106510002,"d":"1.04"},{"$f":"VLOOKUP(A36255,cordwood_density!A:D,4,FALSE)","v":1.1765},{"v":0.8814021340000001,"d":"0.88"}]
["46117","46","SD","117","Stanley","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",29.541141474459998,"A","CEC Survey",2017,15,"I",6.412839197322817,"TON",8,{"v":0.21708163182750004,"d":"0.22"},{"$f":"VLOOKUP(A36294,cordwood_density!A:D,4,FALSE)","v":1.1825},{"v":0.183578547,"d":"0.18"}]
["46119","46","SD","119","Sully","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",66.08914462688,"A","CEC Survey",2017,15,"I",58.38787440962788,"TON",8,{"v":0.883471479912,"d":"0.88"},{"$f":"VLOOKUP(A36315,cordwood_density!A:D,4,FALSE)","v":1.031},{"v":0.8569073520000001,"d":"0.86"}]
["46123","46","SD","123","Tripp","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.597928666249906,"A","CEC Survey",2017,15,"I",5.284789850522793,"TON",8,{"v":2.03423208619171,"d":"2.03"},{"$f":"VLOOKUP(A36333,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.56407203305529,"d":"1.56"}]
["46125","46","SD","125","Turner","","2104008620","Hydronic heater: indoor","Hydronic heater",45.993546076989354,"A","CEC Survey",2017,15,"I",89.08960628981316,"TON",8,{"v":1.9370023381255406,"d":"1.94"},{"$f":"VLOOKUP(A36350,cordwood_density!A:D,4,FALSE)","v":1.2323},{"v":1.5718593995987509,"d":"1.57"}]
["46127","46","SD","127","Union","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",31.180264614,"A","CEC Survey",2017,15,"I",8.633323295794453,"TON",8,{"v":0.2768842215636,"d":"0.28"},{"$f":"VLOOKUP(A36368,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.21288960599999998,"d":"0.21"}]
["46129","46","SD","129","Walworth","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",38.51659279871999,"A","CEC Survey",2017,15,"I",38.19482893297108,"TON",8,{"v":0.9916460973733999,"d":"0.99"},{"$f":"VLOOKUP(A36389,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.7624527889999999,"d":"0.76"}]
["47001","47","TN","001","Anderson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",698.7647960807919,"A","CEC Survey",2017,15,"I",341.3328540093238,"TON",8,{"v":0.4884803240285999,"d":"0.49"},{"$f":"VLOOKUP(A36428,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.406322013,"d":"0.41"}]
["47003","47","TN","003","Bedford","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",506.59028600711997,"A","CEC Survey",2017,15,"I",156.2645658309927,"TON",8,{"v":0.3084634075056,"d":"0.31"},{"$f":"VLOOKUP(A36444,cordwood_density!A:D,4,FALSE)","v":1.2234},{"v":0.252136184,"d":"0.25"}]
["47007","47","TN","007","Bledsoe","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",44.524365809855716,"A","CEC Survey",2017,15,"I",66.08455817479569,"TON",8,{"v":1.4842335645388913,"d":"1.48"},{"$f":"VLOOKUP(A36467,cordwood_density!A:D,4,FALSE)","v":1.2436},{"v":1.1934975591338786,"d":"1.19"}]
["47009","47","TN","009","Blount","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1275.8273880813072,"A","CEC Survey",2017,15,"I",616.4008221517125,"TON",8,{"v":0.48313810152540004,"d":"0.48"},{"$f":"VLOOKUP(A36488,cordwood_density!A:D,4,FALSE)","v":1.2582},{"v":0.383991497,"d":"0.38"}]
["47013","47","TN","013","Campbell","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",413.30835759864,"A","CEC Survey",2017,15,"I",232.15073346714127,"TON",8,{"v":0.5616889404704,"d":"0.56"},{"$f":"VLOOKUP(A36520,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.442135501,"d":"0.44"}]
["47013","47","TN","013","Campbell","","2104009000","Wax Log; Total: All Combustor Types",null,227.55256819472214,"A","CEC Survey",2017,15,"I",78.14809405440319,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A36523,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.27033119489924434,"d":"0.27"}]
["47019","47","TN","019","Carter","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3502.8217418940003,"A","CEC Survey",2017,15,"I",547.215783898438,"TON",8,{"v":0.15622141925000002,"d":"0.16"},{"$f":"VLOOKUP(A36566,cordwood_density!A:D,4,FALSE)","v":1.1806},{"v":0.13232375000000002,"d":"0.13"}]
["47021","47","TN","021","Cheatham","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.007835933077187,"A","CEC Survey",2017,15,"I",16.803106656150813,"TON",8,{"v":1.6789950163565712,"d":"1.68"},{"$f":"VLOOKUP(A36573,cordwood_density!A:D,4,FALSE)","v":1.4689},{"v":1.1430288081942754,"d":"1.14"}]
["47025","47","TN","025","Claiborne","","2104008620","Hydronic heater: indoor","Hydronic heater",65.8027644603371,"A","CEC Survey",2017,15,"I",113.51286595310212,"TON",8,{"v":1.7250470688282784,"d":"1.73"},{"$f":"VLOOKUP(A36605,cordwood_density!A:D,4,FALSE)","v":1.4443},{"v":1.1943827936220166,"d":"1.19"}]
["47027","47","TN","027","Clay","","2104008100","Fireplace: general","Fireplace: general",265.716567417,"A","CEC Survey",2017,15,"I",63.24398979189858,"TON",8,{"v":0.2380129715158,"d":"0.24"},{"$f":"VLOOKUP(A36622,cordwood_density!A:D,4,FALSE)","v":1.2337},{"v":0.192926134,"d":"0.19"}]
["47029","47","TN","029","Cocke","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",580.56978363648,"A","CEC Survey",2017,15,"I",297.32071197690493,"TON",8,{"v":0.5121188190584,"d":"0.51"},{"$f":"VLOOKUP(A36639,cordwood_density!A:D,4,FALSE)","v":1.2886},{"v":0.397422644,"d":"0.40"}]
["47031","47","TN","031","Coffee","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",751.0250465512801,"A","CEC Survey",2017,15,"I",591.9334563372563,"TON",8,{"v":0.7881673974196,"d":"0.79"},{"$f":"VLOOKUP(A36659,cordwood_density!A:D,4,FALSE)","v":1.2998},{"v":0.6063759019999999,"d":"0.61"}]
["47037","47","TN","037","Davidson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",3287.06464247084,"A","CEC Survey",2017,15,"I",1368.312029571542,"TON",8,{"v":0.4162717130329999,"d":"0.42"},{"$f":"VLOOKUP(A36700,cordwood_density!A:D,4,FALSE)","v":1.3331},{"v":0.31225843,"d":"0.31"}]
["47039","47","TN","039","Decatur","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",213.278846625,"A","CEC Survey",2017,15,"I",52.423848577242104,"TON",8,{"v":0.245799569,"d":"0.25"},{"$f":"VLOOKUP(A36717,cordwood_density!A:D,4,FALSE)","v":1.3381},{"v":0.18369297436663926,"d":"0.18"}]
["47041","47","TN","041","Dekalb","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",359.65075866220764,"A","CEC Survey",2017,15,"I",242.16420350102445,"TON",8,{"v":0.6733315519805999,"d":"0.67"},{"$f":"VLOOKUP(A36735,cordwood_density!A:D,4,FALSE)","v":1.0047},{"v":0.6701816979999999,"d":"0.67"}]
["47045","47","TN","045","Dyer","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.5226518081126554,"A","CEC Survey",2017,15,"I",1.6400734199595868,"TON",8,{"v":1.0771165221236474,"d":"1.08"},{"$f":"VLOOKUP(A36756,cordwood_density!A:D,4,FALSE)","v":1.0076},{"v":1.0689921815439136,"d":"1.07"}]
["47047","47","TN","047","Fayette","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",655.779026844,"A","CEC Survey",2017,15,"I",123.70834002379057,"TON",8,{"v":0.188643331,"d":"0.19"},{"$f":"VLOOKUP(A36777,cordwood_density!A:D,4,FALSE)","v":1.3984},{"v":0.13489940717963386,"d":"0.13"}]
["47051","47","TN","051","Franklin","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",628.8106663300001,"A","CEC Survey",2017,15,"I",556.9364044538896,"TON",8,{"v":0.8856980873183998,"d":"0.89"},{"$f":"VLOOKUP(A36811,cordwood_density!A:D,4,FALSE)","v":1.3296},{"v":0.6661387539999999,"d":"0.67"}]
["47055","47","TN","055","Giles","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",384.24048685232,"A","CEC Survey",2017,15,"I",155.15500875442885,"TON",8,{"v":0.40379661712759995,"d":"0.40"},{"$f":"VLOOKUP(A36834,cordwood_density!A:D,4,FALSE)","v":1.3154},{"v":0.306976294,"d":"0.31"}]
["47057","47","TN","057","Grainger","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",670.6729113897632,"A","CEC Survey",2017,15,"I",545.4874320592239,"TON",8,{"v":0.8133434686200001,"d":"0.81"},{"$f":"VLOOKUP(A36855,cordwood_density!A:D,4,FALSE)","v":1.14},{"v":0.7134591830000001,"d":"0.71"}]
["47059","47","TN","059","Greene","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",976.8476769888899,"A","CEC Survey",2017,15,"I",333.3093590206834,"TON",8,{"v":0.3412091433212,"d":"0.34"},{"$f":"VLOOKUP(A36864,cordwood_density!A:D,4,FALSE)","v":1.2313},{"v":0.277112924,"d":"0.28"}]
["47063","47","TN","063","Hamblen","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",690.93098929096,"A","CEC Survey",2017,15,"I",208.64303915429204,"TON",8,{"v":0.30197377507760004,"d":"0.30"},{"$f":"VLOOKUP(A36894,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.251184308,"d":"0.25"}]
["47065","47","TN","065","Hamilton","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,16987.1930675,"A","CEC Survey",2017,15,"I",3008.201995363409,"TON",8,{"v":0.177086466458,"d":"0.18"},{"$f":"VLOOKUP(A36911,cordwood_density!A:D,4,FALSE)","v":1.2694},{"v":0.13950406999999998,"d":"0.14"}]
["47069","47","TN","069","Hardeman","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",182.88993073252976,"A","CEC Survey",2017,15,"I",92.51791671706401,"TON",8,{"v":0.5058666507581999,"d":"0.51"},{"$f":"VLOOKUP(A36940,cordwood_density!A:D,4,FALSE)","v":1.3511},{"v":0.37441096199999996,"d":"0.37"}]
["47071","47","TN","071","Hardin","","2104008620","Hydronic heater: indoor","Hydronic heater",44.061369577460134,"A","CEC Survey",2017,15,"I",62.95727565498895,"TON",8,{"v":1.4288542607444308,"d":"1.43"},{"$f":"VLOOKUP(A36950,cordwood_density!A:D,4,FALSE)","v":1.2884},{"v":1.1090144836575837,"d":"1.11"}]
["47075","47","TN","075","Haywood","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",200.77001965824002,"A","CEC Survey",2017,15,"I",168.97733941474618,"TON",8,{"v":0.841646276184,"d":"0.84"},{"$f":"VLOOKUP(A36989,cordwood_density!A:D,4,FALSE)","v":1.4357},{"v":0.58622712,"d":"0.59"}]
["47077","47","TN","077","Henderson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.0130266211363335,"A","CEC Survey",2017,15,"I",7.3944575116249,"TON",8,{"v":1.4750485226724674,"d":"1.48"},{"$f":"VLOOKUP(A36993,cordwood_density!A:D,4,FALSE)","v":1.3769},{"v":1.0712822446600825,"d":"1.07"}]
["47081","47","TN","081","Hickman","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",263.2704817768184,"A","CEC Survey",2017,15,"I",133.27701250838953,"TON",8,{"v":0.5062360641759,"d":"0.51"},{"$f":"VLOOKUP(A37028,cordwood_density!A:D,4,FALSE)","v":1.3451},{"v":0.376355709,"d":"0.38"}]
["47083","47","TN","083","Houston","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",87.15268301880002,"A","CEC Survey",2017,15,"I",43.67410041666747,"TON",8,{"v":0.5011216970479999,"d":"0.50"},{"$f":"VLOOKUP(A37045,cordwood_density!A:D,4,FALSE)","v":1.3576},{"v":0.36912322999999997,"d":"0.37"}]
["47085","47","TN","085","Humphreys","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",243.93171914048006,"A","CEC Survey",2017,15,"I",232.76218090226735,"TON",8,{"v":0.9542103901962,"d":"0.95"},{"$f":"VLOOKUP(A37066,cordwood_density!A:D,4,FALSE)","v":1.3823},{"v":0.690306294,"d":"0.69"}]
["47091","47","TN","091","Johnson","","2104008100","Fireplace: general","Fireplace: general",748.886738088,"A","CEC Survey",2017,15,"I",163.1385456280925,"TON",8,{"v":0.21784141356889997,"d":"0.22"},{"$f":"VLOOKUP(A37102,cordwood_density!A:D,4,FALSE)","v":1.2221},{"v":0.17825170899999998,"d":"0.18"}]
["47093","47","TN","093","Knox","","2104009000","Wax Log; Total: All Combustor Types",null,2618.5852723865914,"A","CEC Survey",2017,15,"I",899.2974668641366,"TON",8,{"$f":"P37123/J37123","v":{"v":0.34342875,"d":"0.34"}},{"$f":"VLOOKUP(A37123,cordwood_density!A:D,4,FALSE)","v":1.346},{"$f":"S37123/T37123","v":{"v":0.25514765973254083,"d":"0.26"}}]
["47097","47","TN","097","Lauderdale","","2104008610","Hydronic heater: outdoor","Hydronic heater",41.847641695930236,"A","CEC Survey",2017,15,"I",56.49726513024939,"TON",8,{"v":1.3500704661152712,"d":"1.35"},{"$f":"VLOOKUP(A37144,cordwood_density!A:D,4,FALSE)","v":1.287},{"v":1.0490058011773669,"d":"1.05"}]
["47097","47","TN","097","Lauderdale","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",366.05545117599996,"A","CEC Survey",2017,15,"I",284.7559175143626,"TON",8,{"v":0.7779037755059999,"d":"0.78"},{"$f":"VLOOKUP(A37155,cordwood_density!A:D,4,FALSE)","v":1.287},{"v":0.6044318379999999,"d":"0.60"}]
["47101","47","TN","101","Lewis","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",159.69328057111,"A","CEC Survey",2017,15,"I",88.38092991650758,"TON",8,{"v":0.5534417578524999,"d":"0.55"},{"$f":"VLOOKUP(A37179,cordwood_density!A:D,4,FALSE)","v":1.4255},{"v":0.388243955,"d":"0.39"}]
["47103","47","TN","103","Lincoln","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",691.4612831667299,"A","CEC Survey",2017,15,"I",544.4630609213959,"TON",8,{"v":0.7874093230902001,"d":"0.79"},{"$f":"VLOOKUP(A37200,cordwood_density!A:D,4,FALSE)","v":1.2283},{"v":0.6410561940000001,"d":"0.64"}]
["47107","47","TN","107","McMinn","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",718.35766420992,"A","CEC Survey",2017,15,"I",552.2690228252693,"TON",8,{"v":0.7687939453289999,"d":"0.77"},{"$f":"VLOOKUP(A37231,cordwood_density!A:D,4,FALSE)","v":1.2102},{"v":0.635261895,"d":"0.64"}]
["47109","47","TN","109","McNairy","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",402.0144668631,"A","CEC Survey",2017,15,"I",200.81626901208898,"TON",8,{"v":0.4995249812252999,"d":"0.50"},{"$f":"VLOOKUP(A37239,cordwood_density!A:D,4,FALSE)","v":1.3239},{"v":0.3773132269999999,"d":"0.38"}]
["47115","47","TN","115","Marion","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.75431079963251,"A","CEC Survey",2017,15,"I",14.096184721465207,"TON",8,{"v":1.6101992542984582,"d":"1.61"},{"$f":"VLOOKUP(A37278,cordwood_density!A:D,4,FALSE)","v":1.3778},{"v":1.1686741575689203,"d":"1.17"}]
["47115","47","TN","115","Marion","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",470.57885701062,"A","CEC Survey",2017,15,"I",281.6036702960959,"TON",8,{"v":0.5984197251975999,"d":"0.60"},{"$f":"VLOOKUP(A37284,cordwood_density!A:D,4,FALSE)","v":1.3778},{"v":0.43432989199999994,"d":"0.43"}]
["47119","47","TN","119","Maury","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1062.771020792,"A","CEC Survey",2017,15,"I",204.80106531703694,"TON",8,{"v":0.192704789,"d":"0.19"},{"$f":"VLOOKUP(A37317,cordwood_density!A:D,4,FALSE)","v":1.2991},{"v":0.14833714802555614,"d":"0.15"}]
["47121","47","TN","121","Meigs","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",260.47364283864,"A","CEC Survey",2017,15,"I",211.07828700640712,"TON",8,{"v":0.8103633239282001,"d":"0.81"},{"$f":"VLOOKUP(A37334,cordwood_density!A:D,4,FALSE)","v":1.1366},{"v":0.712971427,"d":"0.71"}]
["47123","47","TN","123","Monroe","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",858.67684274456,"A","CEC Survey",2017,15,"I",714.5105465018831,"TON",8,{"v":0.8321064583716,"d":"0.83"},{"$f":"VLOOKUP(A37349,cordwood_density!A:D,4,FALSE)","v":1.1813},{"v":0.704398932,"d":"0.70"}]
["47127","47","TN","127","Moore","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",76.21213507713,"A","CEC Survey",2017,15,"I",32.73724362900683,"TON",8,{"v":0.4295542120145999,"d":"0.43"},{"$f":"VLOOKUP(A37373,cordwood_density!A:D,4,FALSE)","v":1.4181},{"v":0.302908266,"d":"0.30"}]
["47133","47","TN","133","Overton","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",84.37354929013449,"A","CEC Survey",2017,15,"I",110.248253587628,"TON",8,{"v":1.3066684347782789,"d":"1.31"},{"$f":"VLOOKUP(A37412,cordwood_density!A:D,4,FALSE)","v":1.0944},{"v":1.1939587306088073,"d":"1.19"}]
["47133","47","TN","133","Overton","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",614.0770190701681,"A","CEC Survey",2017,15,"I",475.39463663527386,"TON",8,{"v":0.7741612564416002,"d":"0.77"},{"$f":"VLOOKUP(A37425,cordwood_density!A:D,4,FALSE)","v":1.0944},{"v":0.7073841890000001,"d":"0.71"}]
["47137","47","TN","137","Pickett","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,339.46136831999996,"A","CEC Survey",2017,15,"I",58.67185327931854,"TON",8,{"v":0.172838086318,"d":"0.17"},{"$f":"VLOOKUP(A37451,cordwood_density!A:D,4,FALSE)","v":1.3124},{"v":0.131696195,"d":"0.13"}]
["47139","47","TN","139","Polk","","2104009000","Wax Log; Total: All Combustor Types",null,100.87115359663787,"A","CEC Survey",2017,15,"I",34.642054190751345,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A37468,cordwood_density!A:D,4,FALSE)","v":1.152},{"v":0.29811523437500004,"d":"0.30"}]
["47143","47","TN","143","Rhea","","2104008610","Hydronic heater: outdoor","Hydronic heater",83.01890674337824,"A","CEC Survey",2017,15,"I",120.29247686768389,"TON",8,{"v":1.448976884741724,"d":"1.45"},{"$f":"VLOOKUP(A37489,cordwood_density!A:D,4,FALSE)","v":1.2863},{"v":1.1264688523219497,"d":"1.13"}]
["47147","47","TN","147","Robertson","","2104008100","Fireplace: general","Fireplace: general",1928.37732903,"A","CEC Survey",2017,15,"I",434.9089029033764,"TON",8,{"v":0.22553101841439996,"d":"0.23"},{"$f":"VLOOKUP(A37522,cordwood_density!A:D,4,FALSE)","v":1.2328},{"v":0.18294209799999997,"d":"0.18"}]
["47147","47","TN","147","Robertson","","2104009000","Wax Log; Total: All Combustor Types",null,360.0078976078212,"A","CEC Survey",2017,15,"I",123.63706226558202,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A37528,cordwood_density!A:D,4,FALSE)","v":1.2328},{"v":0.27857620863075927,"d":"0.28"}]
["47153","47","TN","153","Sequatchie","","2104008100","Fireplace: general","Fireplace: general",645.9876381,"A","CEC Survey",2017,15,"I",146.18441083379867,"TON",8,{"v":0.22629598805289997,"d":"0.23"},{"$f":"VLOOKUP(A37567,cordwood_density!A:D,4,FALSE)","v":1.2811},{"v":0.176641939,"d":"0.18"}]
["47153","47","TN","153","Sequatchie","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",360.15620229495,"A","CEC Survey",2017,15,"I",330.14674421035465,"TON",8,{"v":0.9166765478607,"d":"0.92"},{"$f":"VLOOKUP(A37575,cordwood_density!A:D,4,FALSE)","v":1.2811},{"v":0.715538637,"d":"0.72"}]
["47157","47","TN","157","Shelby","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",5182.582902876401,"A","CEC Survey",2017,15,"I",2504.859831290006,"TON",8,{"v":0.4833226748577,"d":"0.48"},{"$f":"VLOOKUP(A37606,cordwood_density!A:D,4,FALSE)","v":1.1731},{"v":0.412004667,"d":"0.41"}]
["47161","47","TN","161","Stewart","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.172756748143234,"A","CEC Survey",2017,15,"I",6.751435110838312,"TON",8,{"v":1.6179795560435006,"d":"1.62"},{"$f":"VLOOKUP(A37623,cordwood_density!A:D,4,FALSE)","v":1.3499},{"v":1.1985921594514413,"d":"1.20"}]
["47163","47","TN","163","Sullivan","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2047.9284997808,"A","CEC Survey",2017,15,"I",1359.7681456935263,"TON",8,{"v":0.66397247064,"d":"0.66"},{"$f":"VLOOKUP(A37651,cordwood_density!A:D,4,FALSE)","v":1.2132},{"v":0.5472902,"d":"0.55"}]
["47165","47","TN","165","Sumner","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1938.1266802999803,"A","CEC Survey",2017,15,"I",338.944350013734,"TON",8,{"v":0.174882454,"d":"0.17"},{"$f":"VLOOKUP(A37662,cordwood_density!A:D,4,FALSE)","v":1.3184},{"v":0.13264749241504853,"d":"0.13"}]
["47171","47","TN","171","Unicoi","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.4620554143089566,"A","CEC Survey",2017,15,"I",1.9914287577784173,"TON",8,{"v":1.3620747464757825,"d":"1.36"},{"$f":"VLOOKUP(A37701,cordwood_density!A:D,4,FALSE)","v":1.1823},{"v":1.1520551014765987,"d":"1.15"}]
["47173","47","TN","173","Union","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.7571918184280595,"A","CEC Survey",2017,15,"I",2.3704763175294126,"TON",8,{"v":1.3490139736992302,"d":"1.35"},{"$f":"VLOOKUP(A37716,cordwood_density!A:D,4,FALSE)","v":1.1055},{"v":1.2202749649020626,"d":"1.22"}]
["47175","47","TN","175","Van Buren","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",159.7815713553698,"A","CEC Survey",2017,15,"I",150.07310200278823,"TON",8,{"v":0.9392391170632001,"d":"0.94"},{"$f":"VLOOKUP(A37740,cordwood_density!A:D,4,FALSE)","v":1.2758},{"v":0.7361962040000001,"d":"0.74"}]
["47179","47","TN","179","Washington","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",192.0486452460563,"A","CEC Survey",2017,15,"I",270.65442265297,"TON",8,{"v":1.4093013897921671,"d":"1.41"},{"$f":"VLOOKUP(A37757,cordwood_density!A:D,4,FALSE)","v":1.2736},{"v":1.1065494580654578,"d":"1.11"}]
["47183","47","TN","183","Weakley","","2104008100","Fireplace: general","Fireplace: general",961.6750515680001,"A","CEC Survey",2017,15,"I",257.3704285487072,"TON",8,{"v":0.2676272282712,"d":"0.27"},{"$f":"VLOOKUP(A37792,cordwood_density!A:D,4,FALSE)","v":1.3804},{"v":0.193876578,"d":"0.19"}]
["47183","47","TN","183","Weakley","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1932.992948612,"A","CEC Survey",2017,15,"I",347.4092075796023,"TON",8,{"v":0.17972606047480003,"d":"0.18"},{"$f":"VLOOKUP(A37796,cordwood_density!A:D,4,FALSE)","v":1.3804},{"v":0.130198537,"d":"0.13"}]
["47187","47","TN","187","Williamson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",253.05479822630477,"A","CEC Survey",2017,15,"I",353.33822675846176,"TON",8,{"v":1.396291353631929,"d":"1.40"},{"$f":"VLOOKUP(A37817,cordwood_density!A:D,4,FALSE)","v":1.3371},{"v":1.0442684568333924,"d":"1.04"}]
["47189","47","TN","189","Wilson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1912.03294980115,"A","CEC Survey",2017,15,"I",1265.3089474822852,"TON",8,{"v":0.6617610578384,"d":"0.66"},{"$f":"VLOOKUP(A37845,cordwood_density!A:D,4,FALSE)","v":1.1797},{"v":0.560957072,"d":"0.56"}]
["48003","48","TX","003","Andrews","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",128.53876931788,"A","CEC Survey",2017,15,"I",73.54339747604614,"TON",8,{"v":0.5721495379668001,"d":"0.57"},{"$f":"VLOOKUP(A37874,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.44332057800000013,"d":"0.44"}]
["48007","48","TX","007","Aransas","","2104008620","Hydronic heater: indoor","Hydronic heater",8.483976775977343,"A","CEC Survey",2017,15,"I",9.570378757496547,"TON",8,{"v":1.1280533893722324,"d":"1.13"},{"$f":"VLOOKUP(A37895,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.874053455270597,"d":"0.87"}]
["48009","48","TX","009","Archer","","2104008100","Fireplace: general","Fireplace: general",159.35125234544665,"A","CEC Survey",2017,15,"I",41.309437891108395,"TON",8,{"v":0.25923510034020003,"d":"0.26"},{"$f":"VLOOKUP(A37912,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.20086401700000003,"d":"0.20"}]
["48013","48","TX","013","Atascosa","","2104008100","Fireplace: general","Fireplace: general",720.38746676,"A","CEC Survey",2017,15,"I",167.5218038172524,"TON",8,{"v":0.23254402879979996,"d":"0.23"},{"$f":"VLOOKUP(A37942,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.180182883,"d":"0.18"}]
["48013","48","TX","013","Atascosa","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",389.92890582464,"A","CEC Survey",2017,15,"I",246.44558994991726,"TON",8,{"v":0.6320269830438,"d":"0.63"},{"$f":"VLOOKUP(A37951,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.489715623,"d":"0.49"}]
["48019","48","TX","019","Bandera","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",231.43152607120004,"A","CEC Survey",2017,15,"I",78.14387653266867,"TON",8,{"v":0.3376544149332,"d":"0.34"},{"$f":"VLOOKUP(A37990,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.261625922,"d":"0.26"}]
["48021","48","TX","021","Bastrop","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",858.106049735,"A","CEC Survey",2017,15,"I",88.53371871172905,"TON",8,{"v":0.1031734,"d":"0.10"},{"$f":"VLOOKUP(A38007,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.07994219742755308,"d":"0.08"}]
["48025","48","TX","025","Bee","","2104008610","Hydronic heater: outdoor","Hydronic heater",16.7081616834326,"A","CEC Survey",2017,15,"I",18.67653617513066,"TON",8,{"v":1.1178091599179252,"d":"1.12"},{"$f":"VLOOKUP(A38029,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8661158840213274,"d":"0.87"}]
["48027","48","TX","027","Bell","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",6.20418429069732,"A","CEC Survey",2017,15,"I",7.2049405051883735,"TON",8,{"v":1.1613034312974242,"d":"1.16"},{"$f":"VLOOKUP(A38046,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8998166986652907,"d":"0.90"}]
["48031","48","TX","031","Blanco","","2104009000","Wax Log; Total: All Combustor Types",null,60.75537230724451,"A","CEC Survey",2017,15,"I",14.224795055651462,"TON",8,{"$f":"P38083/J38083","v":{"v":0.2341323,"d":"0.23"}},{"$f":"VLOOKUP(A38083,cordwood_density!A:D,4,FALSE)","v":1.2906},{"$f":"S38083/T38083","v":{"v":0.18141352859135285,"d":"0.18"}}]
["48031","48","TX","031","Blanco","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",247.30403815260001,"A","CEC Survey",2017,15,"I",175.9888740023072,"TON",8,{"v":0.7116296010245999,"d":"0.71"},{"$f":"VLOOKUP(A38085,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.551394391,"d":"0.55"}]
["48037","48","TX","037","Bowie","","2104009000","Wax Log; Total: All Combustor Types",null,476.4341500717748,"A","CEC Survey",2017,15,"I",111.5486233548498,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A38128,cordwood_density!A:D,4,FALSE)","v":1.3883},{"v":0.1686467622271843,"d":"0.17"}]
["48039","48","TX","039","Brazoria","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.220234012649657,"A","CEC Survey",2017,15,"I",4.517918036404823,"TON",8,{"v":1.0705373263337752,"d":"1.07"},{"$f":"VLOOKUP(A38136,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8294880879697623,"d":"0.83"}]
["48043","48","TX","043","Brewster","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.6402628489003745,"A","CEC Survey",2017,15,"I",0.7338710440305689,"TON",8,{"v":1.1462027592120372,"d":"1.15"},{"$f":"VLOOKUP(A38163,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8881161934077462,"d":"0.89"}]
["48045","48","TX","045","Briscoe","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",13.519757193039998,"A","CEC Survey",2017,15,"I",3.0313037746339417,"TON",8,{"v":0.22421288573099996,"d":"0.22"},{"$f":"VLOOKUP(A38184,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.17372763499999996,"d":"0.17"}]
["48049","48","TX","049","Brown","","2104008100","Fireplace: general","Fireplace: general",1019.7585916799999,"A","CEC Survey",2017,15,"I",218.43481514897525,"TON",8,{"v":0.21420247589099997,"d":"0.21"},{"$f":"VLOOKUP(A38212,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.165971235,"d":"0.17"}]
["48049","48","TX","049","Brown","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",353.9318050558,"A","CEC Survey",2017,15,"I",223.33624931480713,"TON",8,{"v":0.6310149190452,"d":"0.63"},{"$f":"VLOOKUP(A38219,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.48893144200000005,"d":"0.49"}]
["48055","48","TX","055","Caldwell","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",373.79390097,"A","CEC Survey",2017,15,"I",30.289755184441805,"TON",8,{"v":0.081033305,"d":"0.08"},{"$f":"VLOOKUP(A38262,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.06278731210289788,"d":"0.06"}]
["48055","48","TX","055","Caldwell","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",420.14511794346004,"A","CEC Survey",2017,15,"I",260.3485827627988,"TON",8,{"v":0.6196634725572,"d":"0.62"},{"$f":"VLOOKUP(A38265,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.480135962,"d":"0.48"}]
["48061","48","TX","061","Cameron","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.0693302746740425,"A","CEC Survey",2017,15,"I",3.282875519556459,"TON",8,{"v":1.0695738893414117,"d":"1.07"},{"$f":"VLOOKUP(A38301,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8287415847988624,"d":"0.83"}]
["48063","48","TX","063","Camp","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",115.07249081680001,"A","CEC Survey",2017,15,"I",42.96722037268894,"TON",8,{"v":0.373392633354,"d":"0.37"},{"$f":"VLOOKUP(A38318,cordwood_density!A:D,4,FALSE)","v":1.3845},{"v":0.269694932,"d":"0.27"}]
["48065","48","TX","065","Carson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",30.2443454544,"A","CEC Survey",2017,15,"I",5.879884568838179,"TON",8,{"v":0.19441269038880002,"d":"0.19"},{"$f":"VLOOKUP(A38335,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.150637448,"d":"0.15"}]
["48071","48","TX","071","Chambers","","2104008610","Hydronic heater: outdoor","Hydronic heater",25.72153575894982,"A","CEC Survey",2017,15,"I",31.294565129735897,"TON",8,{"v":1.2166678313073487,"d":"1.22"},{"$f":"VLOOKUP(A38374,cordwood_density!A:D,4,FALSE)","v":1.3978},{"v":0.8704162478947981,"d":"0.87"}]
["48073","48","TX","073","Cherokee","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2780.118712175,"A","CEC Survey",2017,15,"I",421.9356710195834,"TON",8,{"v":0.1517689403592,"d":"0.15"},{"$f":"VLOOKUP(A38396,cordwood_density!A:D,4,FALSE)","v":1.3187},{"v":0.115089816,"d":"0.12"}]
["48075","48","TX","075","Childress","","2104009000","Wax Log; Total: All Combustor Types",null,32.7763025071234,"A","CEC Survey",2017,15,"I",7.673991091488567,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A38413,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["48077","48","TX","077","Clay","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",167.305534,"A","CEC Survey",2017,15,"I",15.31122861369838,"TON",8,{"v":0.09151657,"d":"0.09"},{"$f":"VLOOKUP(A38427,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.07091009607934294,"d":"0.07"}]
["48081","48","TX","081","Coke","","2104008100","Fireplace: general","Fireplace: general",93.295596542,"A","CEC Survey",2017,15,"I",23.655991406102444,"TON",8,{"v":0.2535595706862,"d":"0.25"},{"$f":"VLOOKUP(A38452,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.196466427,"d":"0.20"}]
["48083","48","TX","083","Coleman","","2104009000","Wax Log; Total: All Combustor Types",null,49.83951345298781,"A","CEC Survey",2017,15,"I",11.669039915628977,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A38473,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["48087","48","TX","087","Collingsworth","","2104009000","Wax Log; Total: All Combustor Types",null,15.78490642214225,"A","CEC Survey",2017,15,"I",3.6957564459009355,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A38503,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["48091","48","TX","091","Comal","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1035.9660927881985,"A","CEC Survey",2017,15,"I",336.5096626454794,"TON",8,{"v":0.3248269079346,"d":"0.32"},{"$f":"VLOOKUP(A38530,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.251686741,"d":"0.25"}]
["48093","48","TX","093","Comanche","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",156.70632063380003,"A","CEC Survey",2017,15,"I",107.27979003163877,"TON",8,{"v":0.6845913400158,"d":"0.68"},{"$f":"VLOOKUP(A38551,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.530444243,"d":"0.53"}]
["48095","48","TX","095","Concho","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.08557849850498604,"A","CEC Survey",2017,15,"I",0.0998563493491697,"TON",8,{"v":1.1668392305732238,"d":"1.17"},{"$f":"VLOOKUP(A38556,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.904106020899755,"d":"0.90"}]
["48099","48","TX","099","Coryell","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",362.11381779552005,"A","CEC Survey",2017,15,"I",102.59424157088297,"TON",8,{"v":0.2833204272498,"d":"0.28"},{"$f":"VLOOKUP(A38590,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.219526133,"d":"0.22"}]
["48101","48","TX","101","Cottle","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",31.081632168000002,"A","CEC Survey",2017,15,"I",2.8371482305396754,"TON",8,{"v":0.091280542,"d":"0.09"},{"$f":"VLOOKUP(A38607,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.07072721369905471,"d":"0.07"}]
["48105","48","TX","105","Crockett","","2104008100","Fireplace: general","Fireplace: general",101.60547363900001,"A","CEC Survey",2017,15,"I",21.993029720648675,"TON",8,{"v":0.216455166567,"d":"0.22"},{"$f":"VLOOKUP(A38632,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.167716695,"d":"0.17"}]
["48107","48","TX","107","Crosby","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.3074890619484881,"A","CEC Survey",2017,15,"I",0.3613298064899708,"TON",8,{"v":1.175098080563602,"d":"1.18"},{"$f":"VLOOKUP(A38646,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.910505253807223,"d":"0.91"}]
["48111","48","TX","111","Dallam","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",65.27654455808,"A","CEC Survey",2017,15,"I",38.330465411636425,"TON",8,{"v":0.587201201766,"d":"0.59"},{"$f":"VLOOKUP(A38685,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.45498311,"d":"0.45"}]
["48115","48","TX","115","Dawson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",10.614971232521738,"A","CEC Survey",2017,15,"I",12.536557939844238,"TON",8,{"v":1.1810260871395692,"d":"1.18"},{"$f":"VLOOKUP(A38702,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9150984713618234,"d":"0.92"}]
["48117","48","TX","117","Deaf Smith","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.0690136350260135,"A","CEC Survey",2017,15,"I",1.2531529672829467,"TON",8,{"v":1.1722516217040133,"d":"1.17"},{"$f":"VLOOKUP(A38718,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9082997223802985,"d":"0.91"}]
["48119","48","TX","119","Delta","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,331.69696582,"A","CEC Survey",2017,15,"I",49.554713079526714,"TON",8,{"v":0.1493975471166,"d":"0.15"},{"$f":"VLOOKUP(A38741,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.115758211,"d":"0.12"}]
["48123","48","TX","123","De Witt","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",19.626460432813438,"A","CEC Survey",2017,15,"I",21.990519258735187,"TON",8,{"v":1.1204526325067399,"d":"1.12"},{"$f":"VLOOKUP(A38762,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8681641349037191,"d":"0.87"}]
["48127","48","TX","127","Dimmit","","2104008610","Hydronic heater: outdoor","Hydronic heater",6.083800736226845,"A","CEC Survey",2017,15,"I",6.801389903818857,"TON",8,{"v":1.117950800610386,"d":"1.12"},{"$f":"VLOOKUP(A38794,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8662256319621773,"d":"0.87"}]
["48129","48","TX","129","Donley","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",38.0489581167,"A","CEC Survey",2017,15,"I",26.886692310751855,"TON",8,{"v":0.7066341272285999,"d":"0.71"},{"$f":"VLOOKUP(A38819,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.547523731,"d":"0.55"}]
["48133","48","TX","133","Eastland","","2104008620","Hydronic heater: indoor","Hydronic heater",14.008318201308507,"A","CEC Survey",2017,15,"I",16.60839660785445,"TON",8,{"v":1.1856096048919755,"d":"1.19"},{"$f":"VLOOKUP(A38840,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9186499340554591,"d":"0.92"}]
["48133","48","TX","133","Eastland","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",232.1991330539274,"A","CEC Survey",2017,15,"I",24.20892255579633,"TON",8,{"v":0.104259315,"d":"0.10"},{"$f":"VLOOKUP(A38847,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.08078360065086007,"d":"0.08"}]
["48137","48","TX","137","Edwards","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",27.70219782319057,"A","CEC Survey",2017,15,"I",19.949713386359132,"TON",8,{"v":0.7201491200693998,"d":"0.72"},{"$f":"VLOOKUP(A38879,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5579955989999998,"d":"0.56"}]
["48139","48","TX","139","Ellis","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1277.958242484,"A","CEC Survey",2017,15,"I",736.7306799413188,"TON",8,{"v":0.5764904168616,"d":"0.58"},{"$f":"VLOOKUP(A38896,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.446684036,"d":"0.45"}]
["48143","48","TX","143","Erath","","2104009000","Wax Log; Total: All Combustor Types",null,198.5968162865886,"A","CEC Survey",2017,15,"I",46.49792936985644,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A38923,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["48145","48","TX","145","Falls","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",91.11272904294289,"A","CEC Survey",2017,15,"I",20.561486370732386,"TON",8,{"v":0.2256708429954,"d":"0.23"},{"$f":"VLOOKUP(A38935,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.174857309,"d":"0.17"}]
["48151","48","TX","151","Fisher","","2104008610","Hydronic heater: outdoor","Hydronic heater",8.895303851430745,"A","CEC Survey",2017,15,"I",10.294118563311699,"TON",8,{"v":1.157253168103523,"d":"1.16"},{"$f":"VLOOKUP(A38974,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.896678419420055,"d":"0.90"}]
["48153","48","TX","153","Floyd","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",61.74815949680001,"A","CEC Survey",2017,15,"I",39.06668805310411,"TON",8,{"v":0.6326777732562,"d":"0.63"},{"$f":"VLOOKUP(A38999,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.490219877,"d":"0.49"}]
["48155","48","TX","155","Foard","","2104009000","Wax Log; Total: All Combustor Types",null,8.071990363279294,"A","CEC Survey",2017,15,"I",1.8899136693324166,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A39013,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["48157","48","TX","157","Fort Bend","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",4184.717539247049,"A","CEC Survey",2017,15,"I",1854.6602801915094,"TON",8,{"v":0.44319843879480003,"d":"0.44"},{"$f":"VLOOKUP(A39030,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.34340495800000004,"d":"0.34"}]
["48163","48","TX","163","Frio","","2104008610","Hydronic heater: outdoor","Hydronic heater",6.9461988512636035,"A","CEC Survey",2017,15,"I",7.830395135480009,"TON",8,{"v":1.1272921065390402,"d":"1.13"},{"$f":"VLOOKUP(A39064,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8734635878963585,"d":"0.87"}]
["48163","48","TX","163","Frio","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",132.6206866581,"A","CEC Survey",2017,15,"I",33.070820003232214,"TON",8,{"v":0.249363963018,"d":"0.25"},{"$f":"VLOOKUP(A39069,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.19321553000000002,"d":"0.19"}]
["48169","48","TX","169","Garza","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.3583076772314413,"A","CEC Survey",2017,15,"I",0.4154061347478078,"TON",8,{"v":1.1593559422381143,"d":"1.16"},{"$f":"VLOOKUP(A39108,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8983077190749376,"d":"0.90"}]
["48171","48","TX","171","Gillespie","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",328.26590438889997,"A","CEC Survey",2017,15,"I",100.73852412018508,"TON",8,{"v":0.30688086326760006,"d":"0.31"},{"$f":"VLOOKUP(A39129,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.23778154600000004,"d":"0.24"}]
["48173","48","TX","173","Glasscock","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.280178840202785,"A","CEC Survey",2017,15,"I",0.36253339344192725,"TON",8,{"v":1.2939356633053964,"d":"1.29"},{"$f":"VLOOKUP(A39138,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.0025845833762563,"d":"1.00"}]
["48175","48","TX","175","Goliad","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",109.7316150115,"A","CEC Survey",2017,15,"I",75.78700277048387,"TON",8,{"v":0.6906578633927998,"d":"0.69"},{"$f":"VLOOKUP(A39164,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5351447879999999,"d":"0.54"}]
["48179","48","TX","179","Gray","","2104008620","Hydronic heater: indoor","Hydronic heater",10.756990553164185,"A","CEC Survey",2017,15,"I",12.50130462752625,"TON",8,{"v":1.1621563266920387,"d":"1.16"},{"$f":"VLOOKUP(A39185,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9004775505129697,"d":"0.90"}]
["48183","48","TX","183","Gregg","","2104008610","Hydronic heater: outdoor","Hydronic heater",87.02896025356956,"A","CEC Survey",2017,15,"I",103.4240611310613,"TON",8,{"v":1.1883867258636962,"d":"1.19"},{"$f":"VLOOKUP(A39214,cordwood_density!A:D,4,FALSE)","v":1.4035},{"v":0.8467308342455976,"d":"0.85"}]
["48183","48","TX","183","Gregg","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",886.5875607261,"A","CEC Survey",2017,15,"I",529.4200912465112,"TON",8,{"v":0.5971436039695,"d":"0.60"},{"$f":"VLOOKUP(A39224,cordwood_density!A:D,4,FALSE)","v":1.4035},{"v":0.425467477,"d":"0.43"}]
["48189","48","TX","189","Hale","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",140.47587661821,"A","CEC Survey",2017,15,"I",27.643418879961374,"TON",8,{"v":0.19678409948699999,"d":"0.20"},{"$f":"VLOOKUP(A39263,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.152474895,"d":"0.15"}]
["48189","48","TX","189","Hale","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",350.96212862100003,"A","CEC Survey",2017,15,"I",23.658057017721642,"TON",8,{"v":0.067409145,"d":"0.07"},{"$f":"VLOOKUP(A39267,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.05223085774058578,"d":"0.05"}]
["48195","48","TX","195","Hansford","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",5.8725732063338265,"A","CEC Survey",2017,15,"I",6.826171663317162,"TON",8,{"v":1.1623817061922426,"d":"1.16"},{"$f":"VLOOKUP(A39302,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9006521820798409,"d":"0.90"}]
["48197","48","TX","197","Hardeman","","2104008610","Hydronic heater: outdoor","Hydronic heater",6.7824464178445645,"A","CEC Survey",2017,15,"I",7.654402762311717,"TON",8,{"v":1.1285607420610124,"d":"1.13"},{"$f":"VLOOKUP(A39319,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8744465690849313,"d":"0.87"}]
["48201","48","TX","201","Harris","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",16182.189154400921,"A","CEC Survey",2017,15,"I",4562.173246931533,"TON",8,{"v":0.2819255913648,"d":"0.28"},{"$f":"VLOOKUP(A39355,cordwood_density!A:D,4,FALSE)","v":1.2996},{"v":0.21693258799999998,"d":"0.22"}]
["48201","48","TX","201","Harris","","2104009000","Wax Log; Total: All Combustor Types",null,40518.0475959196,"A","CEC Survey",2017,15,"I",9486.583675142125,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A39358,cordwood_density!A:D,4,FALSE)","v":1.2996},{"v":0.18015720221606643,"d":"0.18"}]
["48207","48","TX","207","Haskell","","2104008100","Fireplace: general","Fireplace: general",152.02978896,"A","CEC Survey",2017,15,"I",35.32735342950032,"TON",8,{"v":0.232371258759,"d":"0.23"},{"$f":"VLOOKUP(A39397,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.180049015,"d":"0.18"}]
["48209","48","TX","209","Hays","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.2904444459566,"A","CEC Survey",2017,15,"I",11.42241164846247,"TON",8,{"v":1.1100017796559458,"d":"1.11"},{"$f":"VLOOKUP(A39408,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8600664649433952,"d":"0.86"}]
["48211","48","TX","211","Hemphill","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",28.689373027280002,"A","CEC Survey",2017,15,"I",17.50115649088644,"TON",8,{"v":0.6100222711122001,"d":"0.61"},{"$f":"VLOOKUP(A39436,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.4726656370000001,"d":"0.47"}]
["48215","48","TX","215","Hidalgo","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",17.897191307404565,"A","CEC Survey",2017,15,"I",19.219553376602,"TON",8,{"v":1.0738865694892772,"d":"1.07"},{"$f":"VLOOKUP(A39453,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8320831934675943,"d":"0.83"}]
["48219","48","TX","219","Hockley","","2104008610","Hydronic heater: outdoor","Hydronic heater",22.28458821524055,"A","CEC Survey",2017,15,"I",26.753082460468715,"TON",8,{"v":1.2005194891675017,"d":"1.20"},{"$f":"VLOOKUP(A39484,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.930202610543547,"d":"0.93"}]
["48219","48","TX","219","Hockley","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",252.42998359999999,"A","CEC Survey",2017,15,"I",20.356756099991877,"TON",8,{"v":0.08064317799999998,"d":"0.08"},{"$f":"VLOOKUP(A39492,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.062485028668836186,"d":"0.06"}]
["48223","48","TX","223","Hopkins","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.4008161842192286,"A","CEC Survey",2017,15,"I",4.010435553174823,"TON",8,{"v":1.1792567830582565,"d":"1.18"},{"$f":"VLOOKUP(A39513,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.913727555445728,"d":"0.91"}]
["48227","48","TX","227","Howard","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",348.325217464,"A","CEC Survey",2017,15,"I",28.448154175180623,"TON",8,{"v":0.081671245,"d":"0.08"},{"$f":"VLOOKUP(A39552,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.06328160932899426,"d":"0.06"}]
["48229","48","TX","229","Hudspeth","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.2589277499265759,"A","CEC Survey",2017,15,"I",0.31928173722862385,"TON",8,{"v":1.2330920008348372,"d":"1.23"},{"$f":"VLOOKUP(A39558,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9554408808576145,"d":"0.96"}]
["48233","48","TX","233","Hutchinson","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.495441051764419,"A","CEC Survey",2017,15,"I",0.5835684106881049,"TON",8,{"v":1.1778765780708667,"d":"1.18"},{"$f":"VLOOKUP(A39591,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9126581265077225,"d":"0.91"}]
["48235","48","TX","235","Irion","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",15.98929530264,"A","CEC Survey",2017,15,"I",3.6659926214542247,"TON",8,{"v":0.229277935773,"d":"0.23"},{"$f":"VLOOKUP(A39608,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.177652205,"d":"0.18"}]
["48239","48","TX","239","Jackson","","2104008610","Hydronic heater: outdoor","Hydronic heater",11.999903875234855,"A","CEC Survey",2017,15,"I",13.582230277977343,"TON",8,{"v":1.1318615898255702,"d":"1.13"},{"$f":"VLOOKUP(A39634,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8770041762169303,"d":"0.88"}]
["48241","48","TX","241","Jasper","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",62.458927662643625,"A","CEC Survey",2017,15,"I",80.61277295626991,"TON",8,{"v":1.2906525291577173,"d":"1.29"},{"$f":"VLOOKUP(A39647,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.951107243299718,"d":"0.95"}]
["48245","48","TX","245","Jefferson","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,11184.17608374,"A","CEC Survey",2017,15,"I",1830.573958286781,"TON",8,{"v":0.163675352085,"d":"0.16"},{"$f":"VLOOKUP(A39686,cordwood_density!A:D,4,FALSE)","v":1.4055},{"v":0.11645347,"d":"0.12"}]
["48247","48","TX","247","Jim Hogg","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",41.28888819186,"A","CEC Survey",2017,15,"I",9.732360113715723,"TON",8,{"v":0.2357137849896,"d":"0.24"},{"$f":"VLOOKUP(A39699,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.182638916,"d":"0.18"}]
["48251","48","TX","251","Johnson","","2104008620","Hydronic heater: indoor","Hydronic heater",93.93372353092194,"A","CEC Survey",2017,15,"I",113.69277901510623,"TON",8,{"v":1.2103510298692655,"d":"1.21"},{"$f":"VLOOKUP(A39725,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9378204167590776,"d":"0.94"}]
["48253","48","TX","253","Jones","","2104008100","Fireplace: general","Fireplace: general",316.155918155,"A","CEC Survey",2017,15,"I",78.12647094064752,"TON",8,{"v":0.2471137386786,"d":"0.25"},{"$f":"VLOOKUP(A39742,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.191471981,"d":"0.19"}]
["48257","48","TX","257","Kaufman","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",672.7157272968205,"A","CEC Survey",2017,15,"I",164.23015337819555,"TON",8,{"v":0.24413009346179998,"d":"0.24"},{"$f":"VLOOKUP(A39775,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.189160153,"d":"0.19"}]
["48257","48","TX","257","Kaufman","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",975.1244354940254,"A","CEC Survey",2017,15,"I",605.0831650267924,"TON",8,{"v":0.6205189235364,"d":"0.62"},{"$f":"VLOOKUP(A39781,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.48079879400000003,"d":"0.48"}]
["48263","48","TX","263","Kent","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",14.340704190999999,"A","CEC Survey",2017,15,"I",10.078586529713524,"TON",8,{"v":0.7027957899054,"d":"0.70"},{"$f":"VLOOKUP(A39824,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5445496590000001,"d":"0.54"}]
["48265","48","TX","265","Kerr","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.703876382616106,"A","CEC Survey",2017,15,"I",5.634973415501915,"TON",8,{"v":1.1979424961775824,"d":"1.20"},{"$f":"VLOOKUP(A39828,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9282058702755172,"d":"0.93"}]
["48269","48","TX","269","King","","2104008610","Hydronic heater: outdoor","Hydronic heater",0.565708758203109,"A","CEC Survey",2017,15,"I",0.7116253093928326,"TON",8,{"v":1.2579358178105748,"d":"1.26"},{"$f":"VLOOKUP(A39859,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9746907003026305,"d":"0.97"}]
["48271","48","TX","271","Kinney","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",21.5647488,"A","CEC Survey",2017,15,"I",4.46398805346957,"TON",8,{"v":0.20700394402320002,"d":"0.21"},{"$f":"VLOOKUP(A39880,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.160393572,"d":"0.16"}]
["48275","48","TX","275","Knox","","2104008610","Hydronic heater: outdoor","Hydronic heater",6.710720084722288,"A","CEC Survey",2017,15,"I",7.509197872874462,"TON",8,{"v":1.118985411114077,"d":"1.12"},{"$f":"VLOOKUP(A39904,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8670272827476189,"d":"0.87"}]
["48275","48","TX","275","Knox","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",57.96410525023999,"A","CEC Survey",2017,15,"I",40.38368127590572,"TON",8,{"v":0.6967015379873999,"d":"0.70"},{"$f":"VLOOKUP(A39915,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5398276289999999,"d":"0.54"}]
["48281","48","TX","281","Lampasas","","2104009000","Wax Log; Total: All Combustor Types",null,111.28430842471168,"A","CEC Survey",2017,15,"I",26.055251085387123,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A39958,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135287,"d":"0.18"}]
["48283","48","TX","283","La Salle","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",75.18162763746,"A","CEC Survey",2017,15,"I",43.19702795072156,"TON",8,{"v":0.574568938026,"d":"0.57"},{"$f":"VLOOKUP(A39975,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.44519520999999995,"d":"0.45"}]
["48285","48","TX","285","Lavaca","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",338.2709969528,"A","CEC Survey",2017,15,"I",227.63715321165625,"TON",8,{"v":0.6729431587758,"d":"0.67"},{"$f":"VLOOKUP(A39990,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5214188430000001,"d":"0.52"}]
["48289","48","TX","289","Leon","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",233.48656750745,"A","CEC Survey",2017,15,"I",83.71427084727506,"TON",8,{"v":0.358539986865,"d":"0.36"},{"$f":"VLOOKUP(A40014,cordwood_density!A:D,4,FALSE)","v":1.4046},{"v":0.255261275,"d":"0.26"}]
["48291","48","TX","291","Liberty","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3534.7575042,"A","CEC Survey",2017,15,"I",528.2028261487794,"TON",8,{"v":0.149431135098,"d":"0.15"},{"$f":"VLOOKUP(A40031,cordwood_density!A:D,4,FALSE)","v":1.2973},{"v":0.11518626,"d":"0.12"}]
["48295","48","TX","295","Lipscomb","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",37.071510710080005,"A","CEC Survey",2017,15,"I",25.581979029873356,"TON",8,{"v":0.6900711230772,"d":"0.69"},{"$f":"VLOOKUP(A40066,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.534690162,"d":"0.53"}]
["48299","48","TX","299","Llano","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",295.496239744,"A","CEC Survey",2017,15,"I",31.756845548009874,"TON",8,{"v":0.107469542,"d":"0.11"},{"$f":"VLOOKUP(A40092,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.08327099178676585,"d":"0.08"}]
["48303","48","TX","303","Lubbock","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",16.458162802254982,"A","CEC Survey",2017,15,"I",19.279232026658253,"TON",8,{"v":1.1714085137143464,"d":"1.17"},{"$f":"VLOOKUP(A40113,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9076464541409782,"d":"0.91"}]
["48303","48","TX","303","Lubbock","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1713.0280416782498,"A","CEC Survey",2017,15,"I",344.476382534871,"TON",8,{"v":0.2010920861502,"d":"0.20"},{"$f":"VLOOKUP(A40119,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.155812867,"d":"0.16"}]
["48307","48","TX","307","McCulloch","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",62.4134655039,"A","CEC Survey",2017,15,"I",16.3951063563813,"TON",8,{"v":0.2626854032862,"d":"0.26"},{"$f":"VLOOKUP(A40148,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.203537427,"d":"0.20"}]
["48309","48","TX","309","McLennan","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1835.5008724145598,"A","CEC Survey",2017,15,"I",1017.3619087093941,"TON",8,{"v":0.5542693681049999,"d":"0.55"},{"$f":"VLOOKUP(A40169,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.429466425,"d":"0.43"}]
["48313","48","TX","313","Madison","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",86.49941449968001,"A","CEC Survey",2017,15,"I",23.172325698839373,"TON",8,{"$f":"P40195/J40195","v":{"v":0.267889971659,"d":"0.27"}},{"$f":"VLOOKUP(A40195,cordwood_density!A:D,4,FALSE)","v":1.2755},{"$f":"S40195/T40195","v":{"v":0.210027418,"d":"0.21"}}]
["48317","48","TX","317","Martin","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,257.137154685,"A","CEC Survey",2017,15,"I",38.33884758638908,"TON",8,{"v":0.1490988248406,"d":"0.15"},{"$f":"VLOOKUP(A40226,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.115526751,"d":"0.12"}]
["48321","48","TX","321","Matagorda","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",21.967431120797354,"A","CEC Survey",2017,15,"I",24.68272479968775,"TON",8,{"v":1.1236054258670114,"d":"1.12"},{"$f":"VLOOKUP(A40247,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8706070245366585,"d":"0.87"}]
["48323","48","TX","323","Maverick","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2004.4482816959999,"A","CEC Survey",2017,15,"I",294.7652176433345,"TON",8,{"v":0.14705553659579998,"d":"0.15"},{"$f":"VLOOKUP(A40271,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.11394354299999998,"d":"0.11"}]
["48325","48","TX","325","Medina","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2092.8300769439998,"A","CEC Survey",2017,15,"I",312.6316163791493,"TON",8,{"v":0.149382226404,"d":"0.15"},{"$f":"VLOOKUP(A40286,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.11574634,"d":"0.12"}]
["48327","48","TX","327","Menard","","2104009000","Wax Log; Total: All Combustor Types",null,13.84590517829402,"A","CEC Survey",2017,15,"I",3.2417736249758886,"TON",8,{"v":0.2341323,"d":"0.23"},{"$f":"VLOOKUP(A40303,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["48331","48","TX","331","Milam","","2104008610","Hydronic heater: outdoor","Hydronic heater",31.72075502870643,"A","CEC Survey",2017,15,"I",37.74857145156992,"TON",8,{"v":1.1900275203855797,"d":"1.19"},{"$f":"VLOOKUP(A40324,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9220730825860682,"d":"0.92"}]
["48333","48","TX","333","Mills","","2104008100","Fireplace: general","Fireplace: general",130.37887227299998,"A","CEC Survey",2017,15,"I",33.04177065204906,"TON",8,{"v":0.25342887291480004,"d":"0.25"},{"$f":"VLOOKUP(A40342,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.19636515800000004,"d":"0.20"}]
["48337","48","TX","337","Montague","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",216.30020879039037,"A","CEC Survey",2017,15,"I",141.42739136238447,"TON",8,{"v":0.6538476876804,"d":"0.65"},{"$f":"VLOOKUP(A40381,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5066230340000001,"d":"0.51"}]
["48341","48","TX","341","Moore","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.0632766767525896,"A","CEC Survey",2017,15,"I",1.2683608790648082,"TON",8,{"v":1.192879432791263,"d":"1.19"},{"$f":"VLOOKUP(A40398,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9242828396027143,"d":"0.92"}]
["48341","48","TX","341","Moore","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",162.28203775174998,"A","CEC Survey",2017,15,"I",92.86257450430418,"TON",8,{"v":0.572229531936,"d":"0.57"},{"$f":"VLOOKUP(A40410,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.44338256000000004,"d":"0.44"}]
["48345","48","TX","345","Motley","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",24.560206013000002,"A","CEC Survey",2017,15,"I",3.0424770597443382,"TON",8,{"v":0.12387832,"d":"0.12"},{"$f":"VLOOKUP(A40437,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.09598506121183946,"d":"0.10"}]
["48349","48","TX","349","Navarro","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.182853812882114,"A","CEC Survey",2017,15,"I",4.920230319149988,"TON",8,{"v":1.1762855072766216,"d":"1.18"},{"$f":"VLOOKUP(A40458,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9114253116973668,"d":"0.91"}]
["48351","48","TX","351","Newton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",205.90708424921223,"A","CEC Survey",2017,15,"I",172.87570012738345,"TON",8,{"v":0.839581118628,"d":"0.84"},{"$f":"VLOOKUP(A40486,cordwood_density!A:D,4,FALSE)","v":1.3476},{"v":0.62301953,"d":"0.62"}]
["48355","48","TX","355","Nueces","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2716.2955671396503,"A","CEC Survey",2017,15,"I",1241.277887553701,"TON",8,{"$f":"P40515/J40515","v":{"v":0.45697452904979996,"d":"0.46"}},{"$f":"VLOOKUP(A40515,cordwood_density!A:D,4,FALSE)","v":1.2906},{"$f":"S40515/T40515","v":{"v":0.354079133,"d":"0.35"}}]
["48359","48","TX","359","Oldham","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.07888784260363911,"A","CEC Survey",2017,15,"I",0.09228387305486946,"TON",8,{"v":1.169811088871283,"d":"1.17"},{"$f":"VLOOKUP(A40536,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.906408716001304,"d":"0.91"}]
["48359","48","TX","359","Oldham","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",10.824854113639999,"A","CEC Survey",2017,15,"I",2.0956549812277423,"TON",8,{"v":0.19359660270960002,"d":"0.19"},{"$f":"VLOOKUP(A40539,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.15000511600000002,"d":"0.15"}]
["48363","48","TX","363","Palo Pinto","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",393.97818826441,"A","CEC Survey",2017,15,"I",260.66829381443426,"TON",8,{"v":0.6616312820837998,"d":"0.66"},{"$f":"VLOOKUP(A40575,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5126540229999998,"d":"0.51"}]
["48367","48","TX","367","Parker","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",154.71722744928533,"A","CEC Survey",2017,15,"I",189.13070679076387,"TON",8,{"v":1.222428231870681,"d":"1.22"},{"$f":"VLOOKUP(A40592,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9471782363789563,"d":"0.95"}]
["48369","48","TX","369","Parmer","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",40.83271698744001,"A","CEC Survey",2017,15,"I",7.730767103169187,"TON",8,{"v":0.18932776639739995,"d":"0.19"},{"$f":"VLOOKUP(A40615,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.14669747899999996,"d":"0.15"}]
["48371","48","TX","371","Pecos","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,580.8951363799999,"A","CEC Survey",2017,15,"I",86.69935138366704,"TON",8,{"v":0.149251295034,"d":"0.15"},{"$f":"VLOOKUP(A40631,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.11564489,"d":"0.12"}]
["48377","48","TX","377","Presidio","","2104008620","Hydronic heater: indoor","Hydronic heater",3.8220760027589047,"A","CEC Survey",2017,15,"I",4.550052729787225,"TON",8,{"v":1.1904663137265827,"d":"1.19"},{"$f":"VLOOKUP(A40670,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9224130743271213,"d":"0.92"}]
["48379","48","TX","379","Rains","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,653.096871581,"A","CEC Survey",2017,15,"I",97.53939411405153,"TON",8,{"v":0.14934904507799998,"d":"0.15"},{"$f":"VLOOKUP(A40691,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.11572062999999999,"d":"0.12"}]
["48381","48","TX","381","Randall","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",872.90581522028,"A","CEC Survey",2017,15,"I",468.74962334798835,"TON",8,{"v":0.5369990841792,"d":"0.54"},{"$f":"VLOOKUP(A40709,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.41608483199999996,"d":"0.42"}]
["48383","48","TX","383","Reagan","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",21.484515038840005,"A","CEC Survey",2017,15,"I",11.699468393212294,"TON",8,{"v":0.544553524809,"d":"0.54"},{"$f":"VLOOKUP(A40726,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.421938265,"d":"0.42"}]
["48387","48","TX","387","Red River","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",164.96853646672,"A","CEC Survey",2017,15,"I",128.2413559224145,"TON",8,{"v":0.7773685738449,"d":"0.78"},{"$f":"VLOOKUP(A40756,cordwood_density!A:D,4,FALSE)","v":1.4167},{"v":0.5487178469999999,"d":"0.55"}]
["48389","48","TX","389","Reeves","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",44.66080127600001,"A","CEC Survey",2017,15,"I",9.006128958003385,"TON",8,{"v":0.2016562332222,"d":"0.20"},{"$f":"VLOOKUP(A40765,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.156249987,"d":"0.16"}]
["48395","48","TX","395","Robertson","","2104008610","Hydronic heater: outdoor","Hydronic heater",22.70449563885409,"A","CEC Survey",2017,15,"I",26.679849734301488,"TON",8,{"v":1.1750910550351268,"d":"1.18"},{"$f":"VLOOKUP(A40804,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9104998101930318,"d":"0.91"}]
["48397","48","TX","397","Rockwall","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",458.9292009400001,"A","CEC Survey",2017,15,"I",109.3654537510008,"TON",8,{"v":0.23830572020039997,"d":"0.24"},{"$f":"VLOOKUP(A40825,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.184647234,"d":"0.18"}]
["48397","48","TX","397","Rockwall","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",825.70967777555,"A","CEC Survey",2017,15,"I",406.60298846511824,"TON",8,{"v":0.49242851259840004,"d":"0.49"},{"$f":"VLOOKUP(A40830,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.381550064,"d":"0.38"}]
["48403","48","TX","403","Sabine","","2104008610","Hydronic heater: outdoor","Hydronic heater",19.542704977733283,"A","CEC Survey",2017,15,"I",25.561144290517184,"TON",8,{"v":1.3079634738200898,"d":"1.31"},{"$f":"VLOOKUP(A40864,cordwood_density!A:D,4,FALSE)","v":1.3439},{"v":0.9732595236402186,"d":"0.97"}]
["48405","48","TX","405","San Augustine","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.5191268898968209,"A","CEC Survey",2017,15,"I",0.6477980309642141,"TON",8,{"v":1.2478606744739562,"d":"1.25"},{"$f":"VLOOKUP(A40881,cordwood_density!A:D,4,FALSE)","v":1.3245},{"v":0.9421371645707484,"d":"0.94"}]
["48407","48","TX","407","San Jacinto","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",411.24657775320003,"A","CEC Survey",2017,15,"I",318.3964529502272,"TON",8,{"v":0.774222741718,"d":"0.77"},{"$f":"VLOOKUP(A40906,cordwood_density!A:D,4,FALSE)","v":1.297},{"v":0.5969334940000001,"d":"0.60"}]
["48409","48","TX","409","San Patricio","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",609.4455340109799,"A","CEC Survey",2017,15,"I",318.02648497398957,"TON",8,{"v":0.5218292156166,"d":"0.52"},{"$f":"VLOOKUP(A40920,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.404330711,"d":"0.40"}]
["48415","48","TX","415","Scurry","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",128.39083653144,"A","CEC Survey",2017,15,"I",28.206426620379638,"TON",8,{"v":0.21969189844379997,"d":"0.22"},{"$f":"VLOOKUP(A40959,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.17022462299999996,"d":"0.17"}]
["48419","48","TX","419","Shelby","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",43.532452633507376,"A","CEC Survey",2017,15,"I",53.006808700303665,"TON",8,{"v":1.2176389220832409,"d":"1.22"},{"$f":"VLOOKUP(A40982,cordwood_density!A:D,4,FALSE)","v":1.3062},{"v":0.9321994503776151,"d":"0.93"}]
["48421","48","TX","421","Sherman","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.44717083975212696,"A","CEC Survey",2017,15,"I",0.5324278171152449,"TON",8,{"v":1.1906586248118887,"d":"1.19"},{"$f":"VLOOKUP(A40998,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9225620833812868,"d":"0.92"}]
["48423","48","TX","423","Smith","","2104008620","Hydronic heater: indoor","Hydronic heater",127.46399857985733,"A","CEC Survey",2017,15,"I",148.36189448978755,"TON",8,{"v":1.1639513599350761,"d":"1.16"},{"$f":"VLOOKUP(A41015,cordwood_density!A:D,4,FALSE)","v":1.3208},{"v":0.8812472440453333,"d":"0.88"}]
["48427","48","TX","427","Starr","","2104008100","Fireplace: general","Fireplace: general",705.45244896,"A","CEC Survey",2017,15,"I",157.54143304117073,"TON",8,{"v":0.2233197053514,"d":"0.22"},{"$f":"VLOOKUP(A41047,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.173035569,"d":"0.17"}]
["48427","48","TX","427","Starr","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",405.11722589759995,"A","CEC Survey",2017,15,"I",215.14543288944049,"TON",8,{"v":0.5310695747700002,"d":"0.53"},{"$f":"VLOOKUP(A41054,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.4114904500000001,"d":"0.41"}]
["48433","48","TX","433","Stonewall","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",12.074954744580001,"A","CEC Survey",2017,15,"I",2.9904825514494835,"TON",8,{"v":0.24765993866699998,"d":"0.25"},{"$f":"VLOOKUP(A41093,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.191895195,"d":"0.19"}]
["48433","48","TX","433","Stonewall","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",30.32483049282,"A","CEC Survey",2017,15,"I",21.603609709209998,"TON",8,{"v":0.7124066106264,"d":"0.71"},{"$f":"VLOOKUP(A41100,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.551996444,"d":"0.55"}]
["48439","48","TX","439","Tarrant","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",1106.5036136893489,"A","CEC Survey",2017,15,"I",60.81538840746121,"TON",8,{"v":0.05496176212627819,"d":"0.05"},{"$f":"VLOOKUP(A41132,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.042586209612798846,"d":"0.04"}]
["48441","48","TX","441","Taylor","","2104008610","Hydronic heater: outdoor","Hydronic heater",101.45697103109023,"A","CEC Survey",2017,15,"I",118.0572735290811,"TON",8,{"v":1.1636191414871226,"d":"1.16"},{"$f":"VLOOKUP(A41149,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9016109882900377,"d":"0.90"}]
["48443","48","TX","443","Terrell","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",13.497636680920001,"A","CEC Survey",2017,15,"I",9.114794128914381,"TON",8,{"v":0.6752881518732,"d":"0.68"},{"$f":"VLOOKUP(A41176,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5232358220000001,"d":"0.52"}]
["48445","48","TX","445","Terry","","2104009000","Wax Log; Total: All Combustor Types",null,59.49143075569899,"A","CEC Survey",2017,15,"I",20.43106770014126,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A41188,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.266100069735007,"d":"0.27"}]
["48449","48","TX","449","Titus","","2104008610","Hydronic heater: outdoor","Hydronic heater",31.53687657426018,"A","CEC Survey",2017,15,"I",40.0288153001623,"TON",8,{"v":1.269270125908191,"d":"1.27"},{"$f":"VLOOKUP(A41209,cordwood_density!A:D,4,FALSE)","v":1.3883},{"v":0.9142621378003248,"d":"0.91"}]
["48453","48","TX","453","Travis","","2104009000","Wax Log; Total: All Combustor Types",null,6428.306190355238,"A","CEC Survey",2017,15,"I",1505.0741134521097,"TON",8,{"v":0.23413230000000002,"d":"0.23"},{"$f":"VLOOKUP(A41248,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135287,"d":"0.18"}]
["48457","48","TX","457","Tyler","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",261.10951307536,"A","CEC Survey",2017,15,"I",134.73011963045647,"TON",8,{"v":0.5159908501364001,"d":"0.52"},{"$f":"VLOOKUP(A41273,cordwood_density!A:D,4,FALSE)","v":1.3226},{"v":0.3901337140000001,"d":"0.39"}]
["48459","48","TX","459","Upshur","","2104008100","Fireplace: general","Fireplace: general",1267.293365433,"A","CEC Survey",2017,15,"I",307.7225432665364,"TON",8,{"v":0.24281871243080003,"d":"0.24"},{"$f":"VLOOKUP(A41287,cordwood_density!A:D,4,FALSE)","v":1.4212},{"v":0.17085470900000002,"d":"0.17"}]
["48461","48","TX","461","Upton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",31.92532597356,"A","CEC Survey",2017,15,"I",6.419204942896219,"TON",8,{"v":0.20106936255599997,"d":"0.20"},{"$f":"VLOOKUP(A41304,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.15579526,"d":"0.16"}]
["48465","48","TX","465","Val Verde","","2104009000","Wax Log; Total: All Combustor Types",null,218.15918439119073,"A","CEC Survey",2017,15,"I",51.07811160763358,"TON",8,{"v":0.23413229999999996,"d":"0.23"},{"$f":"VLOOKUP(A41338,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18141352859135285,"d":"0.18"}]
["48467","48","TX","467","Van Zandt","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.071161582193634,"A","CEC Survey",2017,15,"I",7.961668059509368,"TON",8,{"v":1.311391230775422,"d":"1.31"},{"$f":"VLOOKUP(A41343,cordwood_density!A:D,4,FALSE)","v":1.4134},{"v":0.9278273884076851,"d":"0.93"}]
["48471","48","TX","471","Walker","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",507.123871254,"A","CEC Survey",2017,15,"I",80.44689345694047,"TON",8,{"v":0.158633616,"d":"0.16"},{"$f":"VLOOKUP(A41382,cordwood_density!A:D,4,FALSE)","v":1.281},{"v":0.12383576580796254,"d":"0.12"}]
["48473","48","TX","473","Waller","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.1723436933385474,"A","CEC Survey",2017,15,"I",1.4056779223330886,"TON",8,{"v":1.1990322721232565,"d":"1.20"},{"$f":"VLOOKUP(A41391,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.9290502650885297,"d":"0.93"}]
["48477","48","TX","477","Washington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.8100324621468887,"A","CEC Survey",2017,15,"I",0.9111539269167603,"TON",8,{"v":1.1248363115002353,"d":"1.12"},{"$f":"VLOOKUP(A41421,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8715607558501746,"d":"0.87"}]
["48479","48","TX","479","Webb","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",1269.79174563835,"A","CEC Survey",2017,15,"I",277.9891079912514,"TON",8,{"v":0.21892496068439998,"d":"0.22"},{"$f":"VLOOKUP(A41438,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.169630374,"d":"0.17"}]
["48483","48","TX","483","Wheeler","","2104008100","Fireplace: general","Fireplace: general",166.957277815,"A","CEC Survey",2017,15,"I",44.08688886677501,"TON",8,{"v":0.2640608989542,"d":"0.26"},{"$f":"VLOOKUP(A41467,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.20460320699999998,"d":"0.20"}]
["48485","48","TX","485","Wichita","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",76.77523574718604,"A","CEC Survey",2017,15,"I",87.99586385402257,"TON",8,{"v":1.146149054413653,"d":"1.15"},{"$f":"VLOOKUP(A41477,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.888074581135637,"d":"0.89"}]
["48489","48","TX","489","Willacy","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",180.28521920562997,"A","CEC Survey",2017,15,"I",99.5669731438358,"TON",8,{"v":0.5522747432238,"d":"0.55"},{"$f":"VLOOKUP(A41520,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.427920923,"d":"0.43"}]
["48493","48","TX","493","Wilson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",376.51448656745,"A","CEC Survey",2017,15,"I",90.47233637846888,"TON",8,{"v":0.24028912460519997,"d":"0.24"},{"$f":"VLOOKUP(A41543,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.18618404199999997,"d":"0.19"}]
["48495","48","TX","495","Winkler","","2104008620","Hydronic heater: indoor","Hydronic heater",2.5192653775548366,"A","CEC Survey",2017,15,"I",2.7505372769363925,"TON",8,{"v":1.0918013248790903,"d":"1.09"},{"$f":"VLOOKUP(A41555,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.8459641444902296,"d":"0.85"}]
["48497","48","TX","497","Wise","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3003.6201856280004,"A","CEC Survey",2017,15,"I",448.27140883863854,"TON",8,{"v":0.149243706306,"d":"0.15"},{"$f":"VLOOKUP(A41576,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.11563901000000001,"d":"0.12"}]
["48499","48","TX","499","Wood","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",548.6296092816001,"A","CEC Survey",2017,15,"I",412.9443552706108,"TON",8,{"v":0.7526833190999997,"d":"0.75"},{"$f":"VLOOKUP(A41596,cordwood_density!A:D,4,FALSE)","v":1.38},{"v":0.5454226949999998,"d":"0.55"}]
["48501","48","TX","501","Yoakum","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",63.42950415984001,"A","CEC Survey",2017,15,"I",38.83775135251376,"TON",8,{"v":0.6122978867159999,"d":"0.61"},{"$f":"VLOOKUP(A41611,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.47442885999999995,"d":"0.47"}]
["48507","48","TX","507","Zavala","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",85.61084796576,"A","CEC Survey",2017,15,"I",49.68772918503625,"TON",8,{"v":0.5803905739248,"d":"0.58"},{"$f":"VLOOKUP(A41654,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.449706008,"d":"0.45"}]
["49001","49","UT","001","Beaver","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",74.31241492836,"A","CEC Survey",2017,15,"I",27.219516652501444,"TON",8,{"v":0.36628491590190004,"d":"0.37"},{"$f":"VLOOKUP(A41671,cordwood_density!A:D,4,FALSE)","v":1.0259},{"v":0.357037641,"d":"0.36"}]
["49003","49","UT","003","Box Elder","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",569.226075185,"A","CEC Survey",2017,15,"I",41.098572886182474,"TON",8,{"v":0.072200791,"d":"0.07"},{"$f":"VLOOKUP(A41682,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.07099389478859391,"d":"0.07"}]
["49007","49","UT","007","Carbon","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",85.80405892268,"A","CEC Survey",2017,15,"I",10.74433292329117,"TON",8,{"v":0.1252194017182,"d":"0.13"},{"$f":"VLOOKUP(A41710,cordwood_density!A:D,4,FALSE)","v":1.0177},{"v":0.123041566,"d":"0.12"}]
["49009","49","UT","009","Daggett","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",6.435704856,"A","CEC Survey",2017,15,"I",2.5248190198454217,"TON",8,{"v":0.39231429600000006,"d":"0.39"},{"$f":"VLOOKUP(A41727,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.3857564365781712,"d":"0.39"}]
["49013","49","UT","013","Duchesne","","2104009000","Wax Log; Total: All Combustor Types",null,125.92681912058076,"A","CEC Survey",2017,15,"I",98.2851771334262,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A41758,cordwood_density!A:D,4,FALSE)","v":1.0533},{"v":0.7409991455425805,"d":"0.74"}]
["49017","49","UT","017","Garfield","","2104009000","Wax Log; Total: All Combustor Types",null,33.25225479834467,"A","CEC Survey",2017,15,"I",25.953198657481146,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A41788,cordwood_density!A:D,4,FALSE)","v":1.0541},{"v":0.7404367707048666,"d":"0.74"}]
["49021","49","UT","021","Iron","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A41809,cordwood_density!A:D,4,FALSE)","v":1.0171},{"$error":"#DIV/0!"}]
["49021","49","UT","021","Iron","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A41811,cordwood_density!A:D,4,FALSE)","v":1.0171},{"$error":"#DIV/0!"}]
["49025","49","UT","025","Kane","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",77.74844917685999,"A","CEC Survey",2017,15,"I",8.975212478381206,"TON",8,{"v":0.11543911902299998,"d":"0.12"},{"$f":"VLOOKUP(A41844,cordwood_density!A:D,4,FALSE)","v":1.0554},{"v":0.109379495,"d":"0.11"}]
["49027","49","UT","027","Millard","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",198.93970540675,"A","CEC Survey",2017,15,"I",74.11361758631631,"TON",8,{"v":0.37254311518550004,"d":"0.37"},{"$f":"VLOOKUP(A41865,cordwood_density!A:D,4,FALSE)","v":1.0259},{"v":0.363137845,"d":"0.36"}]
["49031","49","UT","031","Piute","","2104008100","Fireplace: general","Fireplace: general",55.375370243999996,"A","CEC Survey",2017,15,"I",6.871708872106461,"TON",8,{"v":0.124093235708,"d":"0.12"},{"$f":"VLOOKUP(A41887,cordwood_density!A:D,4,FALSE)","v":1.0529},{"v":0.11785852000000001,"d":"0.12"}]
["49035","49","UT","035","Salt Lake","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",7502.660009614,"A","CEC Survey",2017,15,"I",1323.8918880475512,"TON",8,{"v":0.176456335,"d":"0.18"},{"$f":"VLOOKUP(A41922,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17350672074729598,"d":"0.17"}]
["49039","49","UT","039","Sanpete","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A41943,cordwood_density!A:D,4,FALSE)","v":1.056},{"$error":"#DIV/0!"}]
["49041","49","UT","041","Sevier","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",97.929592627,"A","CEC Survey",2017,15,"I",13.540858081974456,"TON",8,{"v":0.1382713612784,"d":"0.14"},{"$f":"VLOOKUP(A41963,cordwood_density!A:D,4,FALSE)","v":1.0522},{"v":0.131411672,"d":"0.13"}]
["49043","49","UT","043","Summit","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",397.794017244,"A","CEC Survey",2017,15,"I",81.12331538480012,"TON",8,{"v":0.20393297,"d":"0.20"},{"$f":"VLOOKUP(A41982,cordwood_density!A:D,4,FALSE)","v":1.0539},{"v":0.19350315020400416,"d":"0.19"}]
["49045","49","UT","045","Tooele","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",409.56811628652,"A","CEC Survey",2017,15,"I",128.40741096730548,"TON",8,{"v":0.31351906034960003,"d":"0.31"},{"$f":"VLOOKUP(A41999,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.305098346,"d":"0.31"}]
["49047","49","UT","047","Uintah","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",293.41412799328003,"A","CEC Survey",2017,15,"I",111.4285250796475,"TON",8,{"v":0.3797653706784,"d":"0.38"},{"$f":"VLOOKUP(A42016,cordwood_density!A:D,4,FALSE)","v":1.0576},{"v":0.35908223399999994,"d":"0.36"}]
["49051","49","UT","051","Wasatch","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",113.53105300455876,"A","CEC Survey",2017,15,"I",17.99778452906108,"TON",8,{"v":0.15852741653279998,"d":"0.16"},{"$f":"VLOOKUP(A42038,cordwood_density!A:D,4,FALSE)","v":1.0542},{"v":0.15037698399999996,"d":"0.15"}]
["49057","49","UT","057","Weber","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A42077,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$error":"#DIV/0!"}]
["50001","50","VT","001","Addison","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",72.79062978508816,"A","CEC Survey",2017,15,"I",139.52750654184211,"TON",8,{"v":1.916833347283741,"d":"1.92"},{"$f":"VLOOKUP(A42098,cordwood_density!A:D,4,FALSE)","v":1.3635},{"v":1.4058183698450615,"d":"1.41"}]
["50001","50","VT","001","Addison","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1029.0700000000002,"A","CEC Survey",2017,15,"I",3774.1879177317705,"TON",8,{"v":3.667571611,"d":"3.67"},{"$f":"VLOOKUP(A42102,cordwood_density!A:D,4,FALSE)","v":1.3635},{"v":2.6898214968830216,"d":"2.69"}]
["50005","50","VT","005","Caledonia","","2104009000","Wax Log; Total: All Combustor Types",null,286.6278,"A","CEC Survey",2017,15,"I",223.71139278432,"TON",8,{"v":0.7804944,"d":"0.78"},{"$f":"VLOOKUP(A42133,cordwood_density!A:D,4,FALSE)","v":1.2598},{"v":0.6195383394189554,"d":"0.62"}]
["50009","50","VT","009","Essex","","2104008610","Hydronic heater: outdoor","Hydronic heater",43.618193449971606,"A","CEC Survey",2017,15,"I",337.6466599549761,"TON",8,{"v":7.740959293562762,"d":"7.74"},{"$f":"VLOOKUP(A42154,cordwood_density!A:D,4,FALSE)","v":1.2261},{"v":6.313481195304431,"d":"6.31"}]
["50011","50","VT","011","Franklin","","2104009000","Wax Log; Total: All Combustor Types",null,441.9813,"A","CEC Survey",2017,15,"I",344.96392955472,"TON",8,{"v":0.7804944,"d":"0.78"},{"$f":"VLOOKUP(A42178,cordwood_density!A:D,4,FALSE)","v":1.2942},{"v":0.6030709318497914,"d":"0.60"}]
["50015","50","VT","015","Lamoille","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1435.8367589636032,"A","CEC Survey",2017,15,"I",6877.524229923885,"TON",8,{"v":4.789906782222325,"d":"4.79"},{"$f":"VLOOKUP(A42211,cordwood_density!A:D,4,FALSE)","v":1.3144},{"v":3.6441774058295233,"d":"3.64"}]
["50019","50","VT","019","Orleans","","2104008100","Fireplace: general","Fireplace: general",201.48736258759712,"A","CEC Survey",2017,15,"I",180.5308222963635,"TON",8,{"v":0.8959907955412206,"d":"0.90"},{"$f":"VLOOKUP(A42232,cordwood_density!A:D,4,FALSE)","v":1.279},{"v":0.7005401059743711,"d":"0.70"}]
["50021","50","VT","021","Rutland","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1310.6069968402217,"A","CEC Survey",2017,15,"I",5616.173128314307,"TON",8,{"v":4.285169499212573,"d":"4.29"},{"$f":"VLOOKUP(A42254,cordwood_density!A:D,4,FALSE)","v":1.3277},{"v":3.227513368390881,"d":"3.23"}]
["50023","50","VT","023","Washington","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2720.2300542131484,"A","CEC Survey",2017,15,"I",11593.209700917847,"TON",8,{"v":4.261848986986246,"d":"4.26"},{"$f":"VLOOKUP(A42271,cordwood_density!A:D,4,FALSE)","v":1.3207},{"v":3.226962207152454,"d":"3.23"}]
["50027","50","VT","027","Windsor","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",37.46298984066645,"A","CEC Survey",2017,15,"I",292.017024277345,"TON",8,{"v":7.794813641925546,"d":"7.79"},{"$f":"VLOOKUP(A42288,cordwood_density!A:D,4,FALSE)","v":1.3111},{"v":5.945247228987527,"d":"5.95"}]
["51001","51","VA","001","Accomack","","2104008100","Fireplace: general","Fireplace: general",529.2372888880001,"A","CEC Survey",2017,15,"I",252.24915280989353,"TON",8,{"$f":"P42307/J42307","v":{"v":0.4766277019896,"d":"0.48"}},{"$f":"VLOOKUP(A42307,cordwood_density!A:D,4,FALSE)","v":1.2278},{"$f":"S42307/T42307","v":{"v":0.388196532,"d":"0.39"}}]
["51003","51","VA","003","Albemarle","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1084.3153461009774,"A","CEC Survey",2017,15,"I",711.3382091380084,"TON",8,{"v":0.656025216,"d":"0.66"},{"$f":"VLOOKUP(A42327,cordwood_density!A:D,4,FALSE)","v":1.158},{"v":0.5665157305699482,"d":"0.57"}]
["51009","51","VA","009","Amherst","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.385960379200471,"A","CEC Survey",2017,15,"I",9.594057989541744,"TON",8,{"v":2.833482059765624,"d":"2.83"},{"$f":"VLOOKUP(A42366,cordwood_density!A:D,4,FALSE)","v":1.3142},{"v":2.1560508748787277,"d":"2.16"}]
["51011","51","VA","011","Appomattox","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",207.19615392976,"A","CEC Survey",2017,15,"I",197.56749866244624,"TON",8,{"v":0.9535287934419001,"d":"0.95"},{"$f":"VLOOKUP(A42383,cordwood_density!A:D,4,FALSE)","v":1.3767},{"v":0.6926191570000001,"d":"0.69"}]
["51013","51","VA","013","Arlington","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",782.8297418538999,"A","CEC Survey",2017,15,"I",245.00228534822477,"TON",8,{"v":0.3129700779738,"d":"0.31"},{"$f":"VLOOKUP(A42405,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.242499673,"d":"0.24"}]
["51017","51","VA","017","Bath","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",33.318984471203706,"A","CEC Survey",2017,15,"I",101.01720556665128,"TON",8,{"v":3.0318212625584824,"d":"3.03"},{"$f":"VLOOKUP(A42422,cordwood_density!A:D,4,FALSE)","v":1.334},{"v":2.272729582127798,"d":"2.27"}]
["51019","51","VA","019","Bedford","","2104009000","Wax Log; Total: All Combustor Types",null,444.20364050736424,"A","CEC Survey",2017,15,"I",62.188509671031,"TON",8,0.14,{"$f":"VLOOKUP(A42448,cordwood_density!A:D,4,FALSE)","v":1.2347},{"v":0.11338786749817771,"d":"0.11"}]
["51021","51","VA","021","Bland","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,421.69356853,"A","CEC Survey",2017,15,"I",116.92371175086971,"TON",8,{"v":0.277271745354,"d":"0.28"},{"$f":"VLOOKUP(A42461,cordwood_density!A:D,4,FALSE)","v":1.1828},{"v":0.23441980499999998,"d":"0.23"}]
["51027","51","VA","027","Buchanan","","2104008620","Hydronic heater: indoor","Hydronic heater",77.37765152579368,"A","CEC Survey",2017,15,"I",222.06498066365006,"TON",8,{"v":2.8698852483216704,"d":"2.87"},{"$f":"VLOOKUP(A42500,cordwood_density!A:D,4,FALSE)","v":1.2277},{"v":2.3376111821468357,"d":"2.34"}]
["51029","51","VA","029","Buckingham","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,903.607641895,"A","CEC Survey",2017,15,"I",274.5764280598545,"TON",8,{"v":0.3038668724448,"d":"0.30"},{"$f":"VLOOKUP(A42521,cordwood_density!A:D,4,FALSE)","v":1.2931},{"v":0.234991008,"d":"0.23"}]
["51033","51","VA","033","Caroline","","2104008620","Hydronic heater: indoor","Hydronic heater",71.61276141797158,"A","CEC Survey",2017,15,"I",204.86762550970022,"TON",8,{"v":2.860769804895244,"d":"2.86"},{"$f":"VLOOKUP(A42545,cordwood_density!A:D,4,FALSE)","v":1.3295},{"v":2.1517636742348585,"d":"2.15"}]
["51035","51","VA","035","Carroll","","2104008620","Hydronic heater: indoor","Hydronic heater",102.59679717693584,"A","CEC Survey",2017,15,"I",320.05774276724054,"TON",8,{"v":3.1195685593895983,"d":"3.12"},{"$f":"VLOOKUP(A42560,cordwood_density!A:D,4,FALSE)","v":1.3792},{"v":2.2618681550098594,"d":"2.26"}]
["51036","51","VA","036","Charles City","","2104008100","Fireplace: general","Fireplace: general",249.910802635,"A","CEC Survey",2017,15,"I",112.88253535418661,"TON",8,{"v":0.45169130011180003,"d":"0.45"},{"$f":"VLOOKUP(A42577,cordwood_density!A:D,4,FALSE)","v":1.2773},{"v":0.353629766,"d":"0.35"}]
["51037","51","VA","037","Charlotte","","2104009000","Wax Log; Total: All Combustor Types",null,64.53283398970439,"A","CEC Survey",2017,15,"I",9.034596758558616,"TON",8,0.14,{"$f":"VLOOKUP(A42598,cordwood_density!A:D,4,FALSE)","v":1.0896},{"v":0.1284875183553598,"d":"0.13"}]
["51041","51","VA","041","Chesterfield","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",3140.26035584296,"A","CEC Survey",2017,15,"I",3585.6682117610735,"TON",8,{"v":1.1418378750314,"d":"1.14"},{"$f":"VLOOKUP(A42616,cordwood_density!A:D,4,FALSE)","v":1.3313},{"v":0.857686378,"d":"0.86"}]
["51047","51","VA","047","Culpeper","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",341.29450346068,"A","CEC Survey",2017,15,"I",261.06546545543705,"TON",8,{"v":0.7649272484856,"d":"0.76"},{"$f":"VLOOKUP(A42655,cordwood_density!A:D,4,FALSE)","v":1.2744},{"v":0.600225399,"d":"0.60"}]
["51049","51","VA","049","Cumberland","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",236.31959125224,"A","CEC Survey",2017,15,"I",366.63234363423385,"TON",8,{"v":1.5514259384568,"d":"1.55"},{"$f":"VLOOKUP(A42674,cordwood_density!A:D,4,FALSE)","v":1.1967},{"v":1.296420104,"d":"1.30"}]
["51053","51","VA","053","Dinwiddie","","2104008610","Hydronic heater: outdoor","Hydronic heater",98.6579801837393,"A","CEC Survey",2017,15,"I",272.41293795309593,"TON",8,{"v":2.7611850297944245,"d":"2.76"},{"$f":"VLOOKUP(A42694,cordwood_density!A:D,4,FALSE)","v":1.2884},{"v":2.1431116344259737,"d":"2.14"}]
["51057","51","VA","057","Essex","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9506426351591533,"A","CEC Survey",2017,15,"I",2.5223524656715988,"TON",8,{"v":2.6533130036286616,"d":"2.65"},{"$f":"VLOOKUP(A42711,cordwood_density!A:D,4,FALSE)","v":1.2771},{"v":2.077607864402679,"d":"2.08"}]
["51061","51","VA","061","Fauquier","","2104008610","Hydronic heater: outdoor","Hydronic heater",207.96900638713424,"A","CEC Survey",2017,15,"I",615.1497535628497,"TON",8,{"v":2.9578914870504724,"d":"2.96"},{"$f":"VLOOKUP(A42739,cordwood_density!A:D,4,FALSE)","v":1.3776},{"v":2.147133773991342,"d":"2.15"}]
["51061","51","VA","061","Fauquier","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1483.08247432338,"A","CEC Survey",2017,15,"I",2309.9603426431036,"TON",8,{"v":1.5575400442223999,"d":"1.56"},{"$f":"VLOOKUP(A42750,cordwood_density!A:D,4,FALSE)","v":1.3776},{"v":1.1306184989999999,"d":"1.13"}]
["51067","51","VA","067","Franklin","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",982.83473721076,"A","CEC Survey",2017,15,"I",819.0033617921632,"TON",8,{"v":0.833307300591,"d":"0.83"},{"$f":"VLOOKUP(A42789,cordwood_density!A:D,4,FALSE)","v":1.2657},{"v":0.65837663,"d":"0.66"}]
["51071","51","VA","071","Giles","","2104008620","Hydronic heater: indoor","Hydronic heater",52.92659768141354,"A","CEC Survey",2017,15,"I",160.23363413020493,"TON",8,{"v":3.0274690070711814,"d":"3.03"},{"$f":"VLOOKUP(A42815,cordwood_density!A:D,4,FALSE)","v":1.3587},{"v":2.2282100589322007,"d":"2.23"}]
["51073","51","VA","073","Gloucester","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.451903521369193,"A","CEC Survey",2017,15,"I",21.089014636300394,"TON",8,{"v":2.4951792910295802,"d":"2.50"},{"$f":"VLOOKUP(A42828,cordwood_density!A:D,4,FALSE)","v":1.2045},{"v":2.071547771714056,"d":"2.07"}]
["51075","51","VA","075","Goochland","","2104008620","Hydronic heater: indoor","Hydronic heater",64.83957643400605,"A","CEC Survey",2017,15,"I",176.37484174207972,"TON",8,{"v":2.7201726390300323,"d":"2.72"},{"$f":"VLOOKUP(A42845,cordwood_density!A:D,4,FALSE)","v":1.2814},{"v":2.1228130474715408,"d":"2.12"}]
["51077","51","VA","077","Grayson","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1131.574373819915,"A","CEC Survey",2017,15,"I",346.64961359276964,"TON",8,{"v":0.30634275714689996,"d":"0.31"},{"$f":"VLOOKUP(A42866,cordwood_density!A:D,4,FALSE)","v":1.3067},{"v":0.23444000699999998,"d":"0.23"}]
["51081","51","VA","081","Greensville","","2104008610","Hydronic heater: outdoor","Hydronic heater",30.038668540454236,"A","CEC Survey",2017,15,"I",83.09087749625687,"TON",8,{"v":2.766130508892402,"d":"2.77"},{"$f":"VLOOKUP(A42889,cordwood_density!A:D,4,FALSE)","v":1.2871},{"v":2.1491185680152296,"d":"2.15"}]
["51083","51","VA","083","Halifax","","2104008620","Hydronic heater: indoor","Hydronic heater",87.56660791384677,"A","CEC Survey",2017,15,"I",229.2199038921332,"TON",8,{"v":2.617663391936494,"d":"2.62"},{"$f":"VLOOKUP(A42905,cordwood_density!A:D,4,FALSE)","v":1.2018},{"v":2.1781189814748663,"d":"2.18"}]
["51087","51","VA","087","Henrico","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",2584.9478456900997,"A","CEC Survey",2017,15,"I",2439.4550769703983,"TON",8,{"v":0.9437153948918998,"d":"0.94"},{"$f":"VLOOKUP(A42944,cordwood_density!A:D,4,FALSE)","v":1.2669},{"v":0.7449012509999999,"d":"0.74"}]
["51091","51","VA","091","Highland","","2104008620","Hydronic heater: indoor","Hydronic heater",12.899845085990695,"A","CEC Survey",2017,15,"I",39.25152336222061,"TON",8,{"v":3.042790289384792,"d":"3.04"},{"$f":"VLOOKUP(A42965,cordwood_density!A:D,4,FALSE)","v":1.3315},{"v":2.285234915046783,"d":"2.29"}]
["51093","51","VA","093","Isle of Wight","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",333.62955481283996,"A","CEC Survey",2017,15,"I",218.66691616898677,"TON",8,{"v":0.6554183015699999,"d":"0.66"},{"$f":"VLOOKUP(A42983,cordwood_density!A:D,4,FALSE)","v":1.206},{"v":0.543464595,"d":"0.54"}]
["51095","51","VA","095","James City","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",397.8886911216,"A","CEC Survey",2017,15,"I",272.9352620260892,"TON",8,{"v":0.6859588324984,"d":"0.69"},{"$f":"VLOOKUP(A43000,cordwood_density!A:D,4,FALSE)","v":1.1636},{"v":0.589514294,"d":"0.59"}]
["51099","51","VA","099","King George","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",237.59600049136003,"A","CEC Survey",2017,15,"I",159.6112034029919,"TON",8,{"v":0.6717756320515,"d":"0.67"},{"$f":"VLOOKUP(A43030,cordwood_density!A:D,4,FALSE)","v":1.1819},{"v":0.568386185,"d":"0.57"}]
["51101","51","VA","101","King William","","2104008610","Hydronic heater: outdoor","Hydronic heater",59.50514901688826,"A","CEC Survey",2017,15,"I",152.3931240865199,"TON",8,{"v":2.5610073515364014,"d":"2.56"},{"$f":"VLOOKUP(A43039,cordwood_density!A:D,4,FALSE)","v":1.2269},{"v":2.08738067612389,"d":"2.09"}]
["51105","51","VA","105","Lee","","2104009000","Wax Log; Total: All Combustor Types",null,133.25965585499162,"A","CEC Survey",2017,15,"I",18.656351819698827,"TON",8,0.14,{"$f":"VLOOKUP(A43078,cordwood_density!A:D,4,FALSE)","v":1.1933},{"v":0.11732171289700831,"d":"0.12"}]
["51107","51","VA","107","Loudoun","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",29.994968442709265,"A","CEC Survey",2017,15,"I",77.37510905721219,"TON",8,{"v":2.579602949241288,"d":"2.58"},{"$f":"VLOOKUP(A43083,cordwood_density!A:D,4,FALSE)","v":1.2893},{"v":2.000777902149452,"d":"2.00"}]
["51111","51","VA","111","Lunenburg","","2104008100","Fireplace: general","Fireplace: general",417.29806271999996,"A","CEC Survey",2017,15,"I",174.78997909691088,"TON",8,{"v":0.4188612282492,"d":"0.42"},{"$f":"VLOOKUP(A43117,cordwood_density!A:D,4,FALSE)","v":1.2364},{"v":0.33877485300000004,"d":"0.34"}]
["51113","51","VA","113","Madison","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",232.2846828946,"A","CEC Survey",2017,15,"I",232.27451022440047,"TON",8,{"v":0.9999562060224,"d":"1.00"},{"$f":"VLOOKUP(A43134,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.709390044,"d":"0.71"}]
["51117","51","VA","117","Mecklenburg","","2104008610","Hydronic heater: outdoor","Hydronic heater",97.03536593484478,"A","CEC Survey",2017,15,"I",274.3596596247238,"TON",8,{"v":2.827419229901652,"d":"2.83"},{"$f":"VLOOKUP(A43159,cordwood_density!A:D,4,FALSE)","v":1.3146},{"v":2.150782922487184,"d":"2.15"}]
["51119","51","VA","119","Middlesex","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.280688676432953,"A","CEC Survey",2017,15,"I",7.290145154463104,"TON",8,{"v":2.222138664614034,"d":"2.22"},{"$f":"VLOOKUP(A43173,cordwood_density!A:D,4,FALSE)","v":1.0703},{"v":2.076182999732817,"d":"2.08"}]
["51125","51","VA","125","Nelson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",363.32224646256003,"A","CEC Survey",2017,15,"I",604.9557708189302,"TON",8,{"v":1.6650666913711,"d":"1.67"},{"$f":"VLOOKUP(A43216,cordwood_density!A:D,4,FALSE)","v":1.2503},{"v":1.3317337370000002,"d":"1.33"}]
["51131","51","VA","131","Northampton","","2104008620","Hydronic heater: indoor","Hydronic heater",24.02892603821826,"A","CEC Survey",2017,15,"I",61.911347819648384,"TON",8,{"v":2.576534120633512,"d":"2.58"},{"$f":"VLOOKUP(A43235,cordwood_density!A:D,4,FALSE)","v":1.2622},{"v":2.041304167828801,"d":"2.04"}]
["51133","51","VA","133","Northumberland","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.3055541755821085,"A","CEC Survey",2017,15,"I",3.510303564506096,"TON",8,{"v":2.6887459977989456,"d":"2.69"},{"$f":"VLOOKUP(A43251,cordwood_density!A:D,4,FALSE)","v":1.3113},{"v":2.0504430700823195,"d":"2.05"}]
["51135","51","VA","135","Nottoway","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",202.32965968899998,"A","CEC Survey",2017,15,"I",129.970916651588,"TON",8,{"v":0.642372042,"d":"0.64"},{"$f":"VLOOKUP(A43272,cordwood_density!A:D,4,FALSE)","v":1.3954},{"v":0.46034975060914435,"d":"0.46"}]
["51137","51","VA","137","Orange","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",709.1787818442001,"A","CEC Survey",2017,15,"I",1084.441863060897,"TON",8,{"v":1.5291515917056,"d":"1.53"},{"$f":"VLOOKUP(A43289,cordwood_density!A:D,4,FALSE)","v":1.3232},{"v":1.155646608,"d":"1.16"}]
["51141","51","VA","141","Patrick","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",434.97826041852005,"A","CEC Survey",2017,15,"I",686.8411618208057,"TON",8,{"v":1.5790241129751001,"d":"1.58"},{"$f":"VLOOKUP(A43321,cordwood_density!A:D,4,FALSE)","v":1.1681},{"v":1.3517884710000003,"d":"1.35"}]
["51145","51","VA","145","Powhatan","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",880.76290387206,"A","CEC Survey",2017,15,"I",1505.628883534716,"TON",8,{"v":1.7094599203889997,"d":"1.71"},{"$f":"VLOOKUP(A43350,cordwood_density!A:D,4,FALSE)","v":1.3611},{"v":1.25593999,"d":"1.26"}]
["51149","51","VA","149","Prince George","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",82.76037540093226,"A","CEC Survey",2017,15,"I",228.2402413661795,"TON",8,{"v":2.7578444425906805,"d":"2.76"},{"$f":"VLOOKUP(A43367,cordwood_density!A:D,4,FALSE)","v":1.3165},{"v":2.0948305678622714,"d":"2.09"}]
["51149","51","VA","149","Prince George","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",415.02323360316,"A","CEC Survey",2017,15,"I",396.7789439620033,"TON",8,{"v":0.956040317351,"d":"0.96"},{"$f":"VLOOKUP(A43374,cordwood_density!A:D,4,FALSE)","v":1.3165},{"v":0.726198494,"d":"0.73"}]
["51155","51","VA","155","Pulaski","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2178.7779809099998,"A","CEC Survey",2017,15,"I",611.7902407485974,"TON",8,{"v":0.28079512741039997,"d":"0.28"},{"$f":"VLOOKUP(A43406,cordwood_density!A:D,4,FALSE)","v":1.2022},{"v":0.233567732,"d":"0.23"}]
["51157","51","VA","157","Rappahannock","","2104009000","Wax Log; Total: All Combustor Types",null,44.97046588510226,"A","CEC Survey",2017,15,"I",6.2958652239143165,"TON",8,0.14,{"$f":"VLOOKUP(A43423,cordwood_density!A:D,4,FALSE)","v":1.402},{"v":0.09985734664764624,"d":"0.10"}]
["51161","51","VA","161","Roanoke","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",799.7927980442399,"A","CEC Survey",2017,15,"I",944.3339115870153,"TON",8,{"v":1.1807231996790002,"d":"1.18"},{"$f":"VLOOKUP(A43450,cordwood_density!A:D,4,FALSE)","v":1.3422},{"v":0.8796924450000001,"d":"0.88"}]
["51165","51","VA","165","Rockingham","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1565.5398931606499,"A","CEC Survey",2017,15,"I",2561.436415192502,"TON",8,{"v":1.636136151102,"d":"1.64"},{"$f":"VLOOKUP(A43484,cordwood_density!A:D,4,FALSE)","v":1.377},{"v":1.188188926,"d":"1.19"}]
["51169","51","VA","169","Scott","","2104008620","Hydronic heater: indoor","Hydronic heater",65.42070011515308,"A","CEC Survey",2017,15,"I",178.17714183808553,"TON",8,{"v":2.7235590802981213,"d":"2.72"},{"$f":"VLOOKUP(A43505,cordwood_density!A:D,4,FALSE)","v":1.1986},{"v":2.272283564406909,"d":"2.27"}]
["51171","51","VA","171","Shenandoah","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2709.03518739,"A","CEC Survey",2017,15,"I",935.0956438295888,"TON",8,{"v":0.3451766326928001,"d":"0.35"},{"$f":"VLOOKUP(A43526,cordwood_density!A:D,4,FALSE)","v":1.4936},{"v":0.23110379800000005,"d":"0.23"}]
["51173","51","VA","173","Smyth","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",359.19899293348,"A","CEC Survey",2017,15,"I",346.56374825672475,"TON",8,{"v":0.9648238304524,"d":"0.96"},{"$f":"VLOOKUP(A43540,cordwood_density!A:D,4,FALSE)","v":1.3582},{"v":0.710369482,"d":"0.71"}]
["51175","51","VA","175","Southampton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",345.3946202,"A","CEC Survey",2017,15,"I",540.4116183342926,"TON",8,{"v":1.5646208328935998,"d":"1.56"},{"$f":"VLOOKUP(A43561,cordwood_density!A:D,4,FALSE)","v":1.2622},{"v":1.2395981879999998,"d":"1.24"}]
["51179","51","VA","179","Stafford","","2104008610","Hydronic heater: outdoor","Hydronic heater",186.9808212340563,"A","CEC Survey",2017,15,"I",400.27025808967494,"TON",8,{"v":2.1407022145262165,"d":"2.14"},{"$f":"VLOOKUP(A43579,cordwood_density!A:D,4,FALSE)","v":1.0814},{"v":1.9795655765916558,"d":"1.98"}]
["51183","51","VA","183","Sussex","","2104009000","Wax Log; Total: All Combustor Types",null,48.661749734502216,"A","CEC Survey",2017,15,"I",16.71184388413293,"TON",8,{"v":0.34342875,"d":"0.34"},{"$f":"VLOOKUP(A43618,cordwood_density!A:D,4,FALSE)","v":1.264},{"v":0.27169996044303796,"d":"0.27"}]
["51187","51","VA","187","Warren","","2104008610","Hydronic heater: outdoor","Hydronic heater",139.3524434036755,"A","CEC Survey",2017,15,"I",415.715141239697,"TON",8,{"v":2.9831923365380497,"d":"2.98"},{"$f":"VLOOKUP(A43639,cordwood_density!A:D,4,FALSE)","v":1.3584},{"v":2.1961074326693533,"d":"2.20"}]
["51191","51","VA","191","Washington","","2104008620","Hydronic heater: indoor","Hydronic heater",137.6062452990683,"A","CEC Survey",2017,15,"I",407.624579202997,"TON",8,{"v":2.9622534814250683,"d":"2.96"},{"$f":"VLOOKUP(A43655,cordwood_density!A:D,4,FALSE)","v":1.3462},{"v":2.2004557134341614,"d":"2.20"}]
["51193","51","VA","193","Westmoreland","","2104009000","Wax Log; Total: All Combustor Types",null,106.45834975899312,"A","CEC Survey",2017,15,"I",36.56085798479381,"TON",8,{"v":0.34342875000000006,"d":"0.34"},{"$f":"VLOOKUP(A43678,cordwood_density!A:D,4,FALSE)","v":1.2904},{"v":0.26614131277123376,"d":"0.27"}]
["51195","51","VA","195","Wise","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1051.1786375500799,"A","CEC Survey",2017,15,"I",1699.6527772987224,"TON",8,{"v":1.6169019390082005,"d":"1.62"},{"$f":"VLOOKUP(A43695,cordwood_density!A:D,4,FALSE)","v":1.2917},{"v":1.2517627460000003,"d":"1.25"}]
["51199","51","VA","199","York","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",53.339161824453875,"A","CEC Survey",2017,15,"I",149.14885144844033,"TON",8,{"v":2.7962353802879134,"d":"2.80"},{"$f":"VLOOKUP(A43712,cordwood_density!A:D,4,FALSE)","v":1.5347},{"v":1.8220078062734824,"d":"1.82"}]
["51510","51","VA","510","Alexandria City","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",239.49037531608,"A","CEC Survey",2017,15,"I",58.602175753769316,"TON",8,{"v":0.244695327219,"d":"0.24"},{"$f":"VLOOKUP(A43741,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.189598115,"d":"0.19"}]
["51540","51","VA","540","Charlottesville City","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.205432838266883,"A","CEC Survey",2017,15,"I",2.8131215155553881E-5,"TON",8,{"v":5.40420288371639e-06,"d":"0.00"},{"$f":"VLOOKUP(A43773,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":4.1873569531352787E-6,"d":"0.00"}]
["51550","51","VA","550","Chesapeake City","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1937.6226442821298,"A","CEC Survey",2017,15,"I",1489.6251514670219,"TON",8,{"v":0.768790123228,"d":"0.77"},{"$f":"VLOOKUP(A43794,cordwood_density!A:D,4,FALSE)","v":1.181},{"v":0.6509653879999999,"d":"0.65"}]
["51580","51","VA","580","Covington City","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",13.688177289983301,"A","CEC Survey",2017,15,"I",22.871800335197122,"TON",8,{"v":1.670916430336871,"d":"1.67"},{"$f":"VLOOKUP(A43817,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.29468187690754,"d":"1.29"}]
["51580","51","VA","580","Covington City","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",65.0132459358,"A","CEC Survey",2017,15,"I",73.7011694201842,"TON",8,{"v":1.1336331290544,"d":"1.13"},{"$f":"VLOOKUP(A43829,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.878376824,"d":"0.88"}]
["51595","51","VA","595","Emporia City","","2104008620","Hydronic heater: indoor","Hydronic heater",4.704762868462772,"A","CEC Survey",2017,15,"I",10.825964362693126,"TON",8,{"v":2.301064828423624,"d":"2.30"},{"$f":"VLOOKUP(A43850,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.7829419095177623,"d":"1.78"}]
["51600","51","VA","600","Fairfax City","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",79.19810249988001,"A","CEC Survey",2017,15,"I",67.11396975320238,"TON",8,{"v":0.847418910741,"d":"0.85"},{"$f":"VLOOKUP(A43870,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.656608485,"d":"0.66"}]
["51630","51","VA","630","Fredericksburg City","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",20.80328990782426,"A","CEC Survey",2017,15,"I",0.3547863883860641,"TON",8,{"$f":"P43907/J43907","v":{"v":0.017054340441250423,"d":"0.02"}},{"$f":"VLOOKUP(A43907,cordwood_density!A:D,4,FALSE)","v":1.2906},{"$f":"S43907/T43907","v":{"v":0.013214272773322813,"d":"0.01"}}]
["51640","51","VA","640","Galax City","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",71.01617000222,"A","CEC Survey",2017,15,"I",56.10889065438739,"TON",8,{"v":0.7900861261968,"d":"0.79"},{"$f":"VLOOKUP(A43928,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.612185128,"d":"0.61"}]
["51650","51","VA","650","Hampton City","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,26.307019329912155,"A","CEC Survey",2017,15,"I",8.988709454418114,"TON",8,{"v":0.3416848310214143,"d":"0.34"},{"$f":"VLOOKUP(A43946,cordwood_density!A:D,4,FALSE)","v":1.2557},{"v":0.2721070566388582,"d":"0.27"}]
["51670","51","VA","670","Hopewell City","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",26.52584436230735,"A","CEC Survey",2017,15,"I",1.3139374451823869,"TON",8,{"v":0.04953423639360048,"d":"0.05"},{"$f":"VLOOKUP(A43967,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.03838078133705291,"d":"0.04"}]
["51678","51","VA","678","Lexington City","","2104008610","Hydronic heater: outdoor","Hydronic heater",7.473535494543379,"A","CEC Survey",2017,15,"I",1.1182457812136672,"TON",8,{"v":0.14962741289315176,"d":"0.15"},{"$f":"VLOOKUP(A43984,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.11593631868367563,"d":"0.12"}]
["51680","51","VA","680","Lynchburg City","","2104008610","Hydronic heater: outdoor","Hydronic heater",92.997013827271,"A","CEC Survey",2017,15,"I",77.50133659737249,"TON",8,{"v":0.8333744644889396,"d":"0.83"},{"$f":"VLOOKUP(A43999,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.6457263788074846,"d":"0.65"}]
["51683","51","VA","683","Manassas City","","2104009000","Wax Log; Total: All Combustor Types",null,236.0971008,"A","CEC Survey",2017,15,"I",33.053594112,"TON",8,0.14,{"$f":"VLOOKUP(A44023,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.10847667751433443,"d":"0.11"}]
["51700","51","VA","700","Newport News City","","2104008100","Fireplace: general","Fireplace: general",5018.852635564999,"A","CEC Survey",2017,15,"I",882.0601772549328,"TON",8,{"v":0.175749367695,"d":"0.18"},{"$f":"VLOOKUP(A44062,cordwood_density!A:D,4,FALSE)","v":1.3602},{"v":0.129208475,"d":"0.13"}]
["51720","51","VA","720","Norton City","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",7.827290711085094,"A","CEC Survey",2017,15,"I",20.486770611484918,"TON",8,{"v":2.617351439684146,"d":"2.62"},{"$f":"VLOOKUP(A44087,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":2.0280113433164004,"d":"2.03"}]
["51720","51","VA","720","Norton City","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",50.145865054880005,"A","CEC Survey",2017,15,"I",62.32041956321205,"TON",8,{"v":1.2427828195805999,"d":"1.24"},{"$f":"VLOOKUP(A44101,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.962949651,"d":"0.96"}]
["51735","51","VA","735","Poquoson City","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",0.8718985557704689,"A","CEC Survey",2017,15,"I",1.898775782265283,"TON",8,{"v":2.177748511794925,"d":"2.18"},{"$f":"VLOOKUP(A44118,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":1.6873923072949983,"d":"1.69"}]
["51740","51","VA","740","Portsmouth City","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",533.70390919208,"A","CEC Survey",2017,15,"I",300.5388154523684,"TON",8,{"v":0.5631190071425999,"d":"0.56"},{"$f":"VLOOKUP(A44139,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.43632342099999993,"d":"0.44"}]
["51750","51","VA","750","Radford","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",94.4914428720291,"A","CEC Survey",2017,15,"I",87.85500038018318,"TON",8,{"v":0.9297667355886,"d":"0.93"},{"$f":"VLOOKUP(A44161,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.7204143310000001,"d":"0.72"}]
["51775","51","VA","775","Salem City","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0538123174868477,"A","CEC Survey",2017,15,"I",0.35100050907871594,"TON",8,{"v":0.33307687076175846,"d":"0.33"},{"$f":"VLOOKUP(A44196,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.258079087836478,"d":"0.26"}]
["51790","51","VA","790","Staunton City","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",233.816948182,"A","CEC Survey",2017,15,"I",123.2931248047287,"TON",8,{"v":0.527306193,"d":"0.53"},{"$f":"VLOOKUP(A44217,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.40857445606694565,"d":"0.41"}]
["51810","51","VA","810","Virginia Beach City","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",331.8588855161462,"A","CEC Survey",2017,15,"I",111.51458346079689,"TON",8,{"v":0.3360301270443798,"d":"0.34"},{"$f":"VLOOKUP(A44237,cordwood_density!A:D,4,FALSE)","v":1.1558},{"v":0.29073380086899103,"d":"0.29"}]
["51820","51","VA","820","Waynesboro City","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9404227206391059,"A","CEC Survey",2017,15,"I",0.624479580584648,"TON",8,{"v":0.664041358082305,"d":"0.66"},{"$f":"VLOOKUP(A44256,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.5145214304062491,"d":"0.51"}]
["51830","51","VA","830","Williamsburg City","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",48.590817595589996,"A","CEC Survey",2017,15,"I",44.36843374103417,"TON",8,{"v":0.913103255646,"d":"0.91"},{"$f":"VLOOKUP(A44273,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.7075029100000001,"d":"0.71"}]
["51840","51","VA","840","Winchester City","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",109.9064068816,"A","CEC Survey",2017,15,"I",67.27208684927858,"TON",8,{"v":0.6120852164856,"d":"0.61"},{"$f":"VLOOKUP(A44290,cordwood_density!A:D,4,FALSE)","v":1.2906},{"v":0.474264076,"d":"0.47"}]
["53003","53","WA","003","Asotin","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",34.922366693465335,"A","CEC Survey",2017,15,"I",92.07319411818062,"TON",8,{"v":2.636510718943036,"d":"2.64"},{"$f":"VLOOKUP(A44312,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.565697468804044,"d":"2.57"}]
["53007","53","WA","007","Chelan","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3822.97633592,"A","CEC Survey",2017,15,"I",1109.4711111974655,"TON",8,{"v":0.29021134679099997,"d":"0.29"},{"$f":"VLOOKUP(A44351,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.285360223,"d":"0.29"}]
["53009","53","WA","009","Clallam","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4654.664899623001,"A","CEC Survey",2017,15,"I",1366.994525117046,"TON",8,{"v":0.293682693512,"d":"0.29"},{"$f":"VLOOKUP(A44366,cordwood_density!A:D,4,FALSE)","v":1.028},{"v":0.285683554,"d":"0.29"}]
["53013","53","WA","013","Columbia","","2104008620","Hydronic heater: indoor","Hydronic heater",9.538415279034277,"A","CEC Survey",2017,15,"I",27.11829149992032,"TON",8,{"v":2.8430604777218225,"d":"2.84"},{"$f":"VLOOKUP(A44390,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.766699569600839,"d":"2.77"}]
["53015","53","WA","015","Cowlitz","","2104008100","Fireplace: general","Fireplace: general",3953.5184915600003,"A","CEC Survey",2017,15,"I",1320.2046101374353,"TON",8,{"v":0.333931563228,"d":"0.33"},{"$f":"VLOOKUP(A44407,cordwood_density!A:D,4,FALSE)","v":1.028},{"v":0.32483615099999996,"d":"0.32"}]
["53017","53","WA","017","Douglas","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",557.9626674647201,"A","CEC Survey",2017,15,"I",1548.0785801342154,"TON",8,{"v":2.7745200000000003,"d":"2.77"},{"$f":"VLOOKUP(A44431,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.7,"d":"2.70"}]
["53019","53","WA","019","Ferry","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",237.86841759912002,"A","CEC Survey",2017,15,"I",653.1628878854237,"TON",8,{"v":2.7459000000000002,"d":"2.75"},{"$f":"VLOOKUP(A44446,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.7000000000000006,"d":"2.70"}]
["53025","53","WA","025","Grant","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",543.8197153760001,"A","CEC Survey",2017,15,"I",726.4778813764909,"TON",8,{"v":1.33588,"d":"1.34"},{"$f":"VLOOKUP(A44485,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.2999999999999998,"d":"1.30"}]
["53029","53","WA","029","Island","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",214.20614028739155,"A","CEC Survey",2017,15,"I",552.7724811763266,"TON",8,{"v":2.5805631922348002,"d":"2.58"},{"$f":"VLOOKUP(A44507,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.5112526199248735,"d":"2.51"}]
["53031","53","WA","031","Jefferson","","2104008610","Hydronic heater: outdoor","Hydronic heater",175.0887675753245,"A","CEC Survey",2017,15,"I",508.8197281084347,"TON",8,{"v":2.9060672203860056,"d":"2.91"},{"$f":"VLOOKUP(A44524,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.857489892218295,"d":"2.86"}]
["53033","53","WA","033","King","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",14389.514720000001,"A","CEC Survey",2017,15,"I",19827.614318916207,"TON",8,{"v":1.3779209865470852,"d":"1.38"},{"$f":"VLOOKUP(A44545,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.3548878923766816,"d":"1.35"}]
["53035","53","WA","035","Kitsap","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",2619.6923732980003,"A","CEC Survey",2017,15,"I",1708.8070313116734,"TON",8,{"v":0.652293013,"d":"0.65"},{"$f":"VLOOKUP(A44562,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.6347732707279097,"d":"0.63"}]
["53037","53","WA","037","Kittitas","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",741.0632277812401,"A","CEC Survey",2017,15,"I",1507.322605307042,"TON",8,{"v":2.0339999999999994,"d":"2.03"},{"$f":"VLOOKUP(A44581,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9999999999999996,"d":"2.00"}]
["53041","53","WA","041","Lewis","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",9.748307306005685,"A","CEC Survey",2017,15,"I",28.733137960212993,"TON",8,{"v":2.9475002231937473,"d":"2.95"},{"$f":"VLOOKUP(A44601,cordwood_density!A:D,4,FALSE)","v":1.028},{"v":2.867218115947225,"d":"2.87"}]
["53045","53","WA","045","Mason","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1927.15975649508,"A","CEC Survey",2017,15,"I",4012.790119025911,"TON",8,{"v":2.0822301345291483,"d":"2.08"},{"$f":"VLOOKUP(A44640,cordwood_density!A:D,4,FALSE)","v":1.028},{"v":2.025515695067265,"d":"2.03"}]
["53049","53","WA","049","Pacific","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",105.20150168064734,"A","CEC Survey",2017,15,"I",305.8559977095672,"TON",8,{"v":2.9073349032415177,"d":"2.91"},{"$f":"VLOOKUP(A44657,cordwood_density!A:D,4,FALSE)","v":1.0281},{"v":2.8278717082399742,"d":"2.83"}]
["53051","53","WA","051","Pend Oreille","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",242.2083206724,"A","CEC Survey",2017,15,"I",418.7539656105123,"TON",8,{"v":1.7288999999999999,"d":"1.73"},{"$f":"VLOOKUP(A44679,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7,"d":"1.70"}]
["53053","53","WA","053","Pierce","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,38033.925033671,"A","CEC Survey",2017,15,"I",11476.650517897187,"TON",8,{"v":0.3017477293689,"d":"0.30"},{"$f":"VLOOKUP(A44696,cordwood_density!A:D,4,FALSE)","v":1.0281},{"v":0.293500369,"d":"0.29"}]
["53057","53","WA","057","Skagit","","2104008100","Fireplace: general","Fireplace: general",5922.35151108,"A","CEC Survey",2017,15,"I",2111.5233035198617,"TON",8,{"v":0.35653461291000005,"d":"0.36"},{"$f":"VLOOKUP(A44722,cordwood_density!A:D,4,FALSE)","v":1.0275},{"v":0.346992324,"d":"0.35"}]
["53059","53","WA","059","Skamania","","2104008620","Hydronic heater: indoor","Hydronic heater",82.7202515735105,"A","CEC Survey",2017,15,"I",267.19281243853544,"TON",8,{"v":3.230077367464131,"d":"3.23"},{"$f":"VLOOKUP(A44735,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":3.1433216888518207,"d":"3.14"}]
["53063","53","WA","063","Spokane","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",7079.983050000001,"A","CEC Survey",2017,15,"I",19643.554571886005,"TON",8,{"v":2.7745200000000003,"d":"2.77"},{"$f":"VLOOKUP(A44774,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":2.7,"d":"2.70"}]
["53067","53","WA","067","Thurston","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",2176.42844397612,"A","CEC Survey",2017,15,"I",4417.233728410368,"TON",8,{"v":2.0295791210762335,"d":"2.03"},{"$f":"VLOOKUP(A44798,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.9750672645739913,"d":"1.98"}]
["53069","53","WA","069","Wahkiakum","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",58.443861701850004,"A","CEC Survey",2017,15,"I",118.61644146514168,"TON",8,{"v":2.0295791210762335,"d":"2.03"},{"$f":"VLOOKUP(A44813,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.9750672645739913,"d":"1.98"}]
["53071","53","WA","071","Walla Walla","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",288.73189369920004,"A","CEC Survey",2017,15,"I",504.39151974100656,"TON",8,{"v":1.74692,"d":"1.75"},{"$f":"VLOOKUP(A44830,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7,"d":"1.70"}]
["53073","53","WA","073","Whatcom","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",2943.13908,"A","CEC Survey",2017,15,"I",6062.717764094029,"TON",8,{"v":2.0599494618834084,"d":"2.06"},{"$f":"VLOOKUP(A44851,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":2.025515695067265,"d":"2.03"}]
["53077","53","WA","077","Yakima","","2104008610","Hydronic heater: outdoor","Hydronic heater",0,"A","CEC Survey",2017,15,"I",0,"TON",8,{"$error":"#DIV/0!"},{"$f":"VLOOKUP(A44869,cordwood_density!A:D,4,FALSE)","v":1.0279},{"$error":"#DIV/0!"}]
["54005","54","WV","005","Boone","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",86.54918099204963,"A","CEC Survey",2017,15,"I",639.1282025266564,"TON",8,{"v":7.384566730739676,"d":"7.38"},{"$f":"VLOOKUP(A44912,cordwood_density!A:D,4,FALSE)","v":1.2689},{"v":5.8196601235240575,"d":"5.82"}]
["54007","54","WV","007","Braxton","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",78.83064267987854,"A","CEC Survey",2017,15,"I",590.3402196092063,"TON",8,{"v":7.488715042023756,"d":"7.49"},{"$f":"VLOOKUP(A44927,cordwood_density!A:D,4,FALSE)","v":1.2761},{"v":5.86843902674066,"d":"5.87"}]
["54009","54","WV","009","Brooke","","2104008100","Fireplace: general","Fireplace: general",1700.302268301,"A","CEC Survey",2017,15,"I",1562.6984417427698,"TON",8,{"v":0.9190709621909,"d":"0.92"},{"$f":"VLOOKUP(A44947,cordwood_density!A:D,4,FALSE)","v":1.2577},{"v":0.730755317,"d":"0.73"}]
["54011","54","WV","011","Cabell","","2104009000","Wax Log; Total: All Combustor Types",null,577.9516374163621,"A","CEC Survey",2017,15,"I",80.91322923829071,"TON",8,0.14,{"$f":"VLOOKUP(A44968,cordwood_density!A:D,4,FALSE)","v":1.3004},{"v":0.10765918179021841,"d":"0.11"}]
["54013","54","WV","013","Calhoun","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",156.43734247439997,"A","CEC Survey",2017,15,"I",780.0298985581335,"TON",8,{"v":4.986212922185,"d":"4.99"},{"$f":"VLOOKUP(A44985,cordwood_density!A:D,4,FALSE)","v":1.315},{"v":3.791796899,"d":"3.79"}]
["54017","54","WV","017","Doddridge","","2104009000","Wax Log; Total: All Combustor Types",null,38.23423191988877,"A","CEC Survey",2017,15,"I",5.352792468784428,"TON",8,0.14,{"$f":"VLOOKUP(A45013,cordwood_density!A:D,4,FALSE)","v":1.3189},{"v":0.10614906361361742,"d":"0.11"}]
["54021","54","WV","021","Gilmer","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",87.59282820540001,"A","CEC Survey",2017,15,"I",423.4539443325737,"TON",8,{"v":4.8343449230752,"d":"4.83"},{"$f":"VLOOKUP(A45046,cordwood_density!A:D,4,FALSE)","v":1.3232},{"v":3.6535254860000004,"d":"3.65"}]
["54025","54","WV","025","Greenbrier","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",17.410605300896453,"A","CEC Survey",2017,15,"I",136.10739755656414,"TON",8,{"v":7.817499461064465,"d":"7.82"},{"$f":"VLOOKUP(A45063,cordwood_density!A:D,4,FALSE)","v":1.2623},{"v":6.193059859830837,"d":"6.19"}]
["54027","54","WV","027","Hampshire","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",679.0219305082001,"A","CEC Survey",2017,15,"I",3015.2487022601813,"TON",8,{"v":4.440576315412199,"d":"4.44"},{"$f":"VLOOKUP(A45089,cordwood_density!A:D,4,FALSE)","v":1.2003},{"v":3.699555373999999,"d":"3.70"}]
["54029","54","WV","029","Hancock","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",395.47478872,"A","CEC Survey",2017,15,"I",564.277219938003,"TON",8,{"v":1.426834873,"d":"1.43"},{"$f":"VLOOKUP(A45102,cordwood_density!A:D,4,FALSE)","v":1.2577},{"v":1.1344795046513476,"d":"1.13"}]
["54031","54","WV","031","Hardy","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",352.23809176055,"A","CEC Survey",2017,15,"I",1612.5254391130652,"TON",8,{"v":4.5779416730694,"d":"4.58"},{"$f":"VLOOKUP(A45119,cordwood_density!A:D,4,FALSE)","v":1.2654},{"v":3.617782261,"d":"3.62"}]
["54035","54","WV","035","Jackson","","2104008100","Fireplace: general","Fireplace: general",1686.767351648,"A","CEC Survey",2017,15,"I",1656.3928903899678,"TON",8,{"v":0.9819925010830001,"d":"0.98"},{"$f":"VLOOKUP(A45142,cordwood_density!A:D,4,FALSE)","v":1.1855},{"v":0.828336146,"d":"0.83"}]
["54039","54","WV","039","Kanawha","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",3038.84759219723,"A","CEC Survey",2017,15,"I",10887.906199890667,"TON",8,{"v":3.5829063056163992,"d":"3.58"},{"$f":"VLOOKUP(A45180,cordwood_density!A:D,4,FALSE)","v":1.2284},{"v":2.9167260709999994,"d":"2.92"}]
["54043","54","WV","043","Lincoln","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.530683150832933,"A","CEC Survey",2017,15,"I",18.412490383239543,"TON",8,{"v":7.275699598023313,"d":"7.28"},{"$f":"VLOOKUP(A45201,cordwood_density!A:D,4,FALSE)","v":1.2723},{"v":5.718540908609064,"d":"5.72"}]
["54045","54","WV","045","Logan","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",395.96363548325996,"A","CEC Survey",2017,15,"I",1066.67452925619,"TON",8,{"v":2.6938699255914007,"d":"2.69"},{"$f":"VLOOKUP(A45218,cordwood_density!A:D,4,FALSE)","v":1.2813},{"v":2.1024505780000005,"d":"2.10"}]
["54047","54","WV","047","McDowell","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1247.18346609993,"A","CEC Survey",2017,15,"I",997.3077772589861,"TON",8,{"v":0.7996480103907,"d":"0.80"},{"$f":"VLOOKUP(A45236,cordwood_density!A:D,4,FALSE)","v":1.2763},{"v":0.626536089,"d":"0.63"}]
["54051","54","WV","051","Marshall","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",109.92041010687218,"A","CEC Survey",2017,15,"I",777.8027337416316,"TON",8,{"v":7.076053782781544,"d":"7.08"},{"$f":"VLOOKUP(A45257,cordwood_density!A:D,4,FALSE)","v":1.2614},{"v":5.609682719820473,"d":"5.61"}]
["54051","54","WV","051","Marshall","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",428.2197721102001,"A","CEC Survey",2017,15,"I",1704.6255881868508,"TON",8,{"v":3.9807260178265995,"d":"3.98"},{"$f":"VLOOKUP(A45271,cordwood_density!A:D,4,FALSE)","v":1.2614},{"v":3.1557999189999992,"d":"3.16"}]
["54055","54","WV","055","Mercer","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3568.2487095640004,"A","CEC Survey",2017,15,"I",2860.360198858233,"TON",8,{"v":0.8016145822996,"d":"0.80"},{"$f":"VLOOKUP(A45296,cordwood_density!A:D,4,FALSE)","v":1.2746},{"v":0.628914626,"d":"0.63"}]
["54061","54","WV","061","Monongalia","","2104008620","Hydronic heater: indoor","Hydronic heater",108.98717710498148,"A","CEC Survey",2017,15,"I",759.6597395335448,"TON",8,{"v":6.970175388631319,"d":"6.97"},{"$f":"VLOOKUP(A45335,cordwood_density!A:D,4,FALSE)","v":1.274},{"v":5.471095281500251,"d":"5.47"}]
["54063","54","WV","063","Monroe","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",81.32070799210808,"A","CEC Survey",2017,15,"I",623.8376756413136,"TON",8,{"v":7.6713261731791,"d":"7.67"},{"$f":"VLOOKUP(A45347,cordwood_density!A:D,4,FALSE)","v":1.2586},{"v":6.0951264684404105,"d":"6.10"}]
["54065","54","WV","065","Morgan","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",510.33992527074,"A","CEC Survey",2017,15,"I",2389.2981114336408,"TON",8,{"v":4.681777758552001,"d":"4.68"},{"$f":"VLOOKUP(A45374,cordwood_density!A:D,4,FALSE)","v":1.2732},{"v":3.6771738600000003,"d":"3.68"}]
["54067","54","WV","067","Nicholas","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",568.99770763668,"A","CEC Survey",2017,15,"I",2657.638014308985,"TON",8,{"v":4.670735889864,"d":"4.67"},{"$f":"VLOOKUP(A45391,cordwood_density!A:D,4,FALSE)","v":1.243},{"v":3.7576314479999997,"d":"3.76"}]
["54071","54","WV","071","Pendleton","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.283052435763,"A","CEC Survey",2017,15,"I",32.74436527706067,"TON",8,{"v":7.645100256921664,"d":"7.65"},{"$f":"VLOOKUP(A45408,cordwood_density!A:D,4,FALSE)","v":1.2196},{"v":6.26853087645266,"d":"6.27"}]
["54073","54","WV","073","Pleasants","","2104009000","Wax Log; Total: All Combustor Types",null,41.19300420264238,"A","CEC Survey",2017,15,"I",5.767020588369934,"TON",8,0.14,{"$f":"VLOOKUP(A45433,cordwood_density!A:D,4,FALSE)","v":1.254},{"v":0.1116427432216906,"d":"0.11"}]
["54079","54","WV","079","Putnam","","2104008610","Hydronic heater: outdoor","Hydronic heater",142.27123757561094,"A","CEC Survey",2017,15,"I",927.7126096589718,"TON",8,{"v":6.520731986786388,"d":"6.52"},{"$f":"VLOOKUP(A45469,cordwood_density!A:D,4,FALSE)","v":1.1523},{"v":5.658883959720895,"d":"5.66"}]
["54081","54","WV","081","Raleigh","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",728.6068750651601,"A","CEC Survey",2017,15,"I",1960.7745389544039,"TON",8,{"v":2.6911282422075,"d":"2.69"},{"$f":"VLOOKUP(A45490,cordwood_density!A:D,4,FALSE)","v":1.2525},{"v":2.148605383,"d":"2.15"}]
["54083","54","WV","083","Randolph","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",546.03716426145,"A","CEC Survey",2017,15,"I",2476.5547529247597,"TON",8,{"v":4.535505850182299,"d":"4.54"},{"$f":"VLOOKUP(A45509,cordwood_density!A:D,4,FALSE)","v":1.2663},{"v":3.5816993209999994,"d":"3.58"}]
["54085","54","WV","085","Ritchie","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",204.37147480725,"A","CEC Survey",2017,15,"I",981.5055222197241,"TON",8,{"v":4.8025563408270004,"d":"4.80"},{"$f":"VLOOKUP(A45525,cordwood_density!A:D,4,FALSE)","v":1.2853},{"v":3.73652559,"d":"3.74"}]
["54089","54","WV","089","Summers","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.9462380090898395,"A","CEC Survey",2017,15,"I",14.889501554952178,"TON",8,{"v":7.65040117673751,"d":"7.65"},{"$f":"VLOOKUP(A45546,cordwood_density!A:D,4,FALSE)","v":1.2768},{"v":5.991855558221735,"d":"5.99"}]
["54091","54","WV","091","Taylor","","2104008100","Fireplace: general","Fireplace: general",1225.3471570572096,"A","CEC Survey",2017,15,"I",1187.218276260401,"TON",8,{"v":0.9688832013220001,"d":"0.97"},{"$f":"VLOOKUP(A45562,cordwood_density!A:D,4,FALSE)","v":1.2515},{"v":0.774177548,"d":"0.77"}]
["54097","54","WV","097","Upshur","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.05450929620218,"A","CEC Survey",2017,15,"I",58.098700634719094,"TON",8,{"v":7.213189345018633,"d":"7.21"},{"$f":"VLOOKUP(A45603,cordwood_density!A:D,4,FALSE)","v":1.2616},{"v":5.717493139678688,"d":"5.72"}]
["54099","54","WV","099","Wayne","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",556.4464616421,"A","CEC Survey",2017,15,"I",1594.360171297199,"TON",8,{"v":2.8652534991276006,"d":"2.87"},{"$f":"VLOOKUP(A45624,cordwood_density!A:D,4,FALSE)","v":1.3116},{"v":2.184548261,"d":"2.18"}]
["54101","54","WV","101","Webster","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",141.88140818280002,"A","CEC Survey",2017,15,"I",435.9559978399202,"TON",8,{"v":3.0726788197522996,"d":"3.07"},{"$f":"VLOOKUP(A45638,cordwood_density!A:D,4,FALSE)","v":1.2331},{"v":2.4918326329999996,"d":"2.49"}]
["54105","54","WV","105","Wirt","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.7854919913309644,"A","CEC Survey",2017,15,"I",19.04166316888541,"TON",8,{"v":6.836014330016766,"d":"6.84"},{"$f":"VLOOKUP(A45663,cordwood_density!A:D,4,FALSE)","v":1.1876},{"v":5.756158917157937,"d":"5.76"}]
["54107","54","WV","107","Wood","","2104008620","Hydronic heater: indoor","Hydronic heater",142.057337883935,"A","CEC Survey",2017,15,"I",860.8911852388891,"TON",8,{"v":6.06016695837467,"d":"6.06"},{"$f":"VLOOKUP(A45680,cordwood_density!A:D,4,FALSE)","v":1.1516},{"v":5.262388814149592,"d":"5.26"}]
["55001","55","WI","001","Adams","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",314.38293103899,"A","CEC Survey",2017,15,"I",261.36504425920384,"TON",8,{"v":0.8313588889683999,"d":"0.83"},{"$f":"VLOOKUP(A45714,cordwood_density!A:D,4,FALSE)","v":1.4186},{"v":0.5860417939999999,"d":"0.59"}]
["55001","55","WI","001","Adams","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",219.06376052291998,"A","CEC Survey",2017,15,"I",589.8698448037885,"TON",8,{"v":2.6926856518656,"d":"2.69"},{"$f":"VLOOKUP(A45719,cordwood_density!A:D,4,FALSE)","v":1.4186},{"v":1.898128896,"d":"1.90"}]
["55007","55","WI","007","Bayfield","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",71.12857845408,"A","CEC Survey",2017,15,"I",71.21859936011587,"TON",8,{"v":1.0012656081140998,"d":"1.00"},{"$f":"VLOOKUP(A45758,cordwood_density!A:D,4,FALSE)","v":1.2327},{"v":0.8122540829999999,"d":"0.81"}]
["55009","55","WI","009","Brown","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",912.5042848530001,"A","CEC Survey",2017,15,"I",1587.9897439562683,"TON",8,{"v":1.7402545613384004,"d":"1.74"},{"$f":"VLOOKUP(A45779,cordwood_density!A:D,4,FALSE)","v":1.3357},{"v":1.3028783120000003,"d":"1.30"}]
["55013","55","WI","013","Burnett","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",290.3599537055585,"A","CEC Survey",2017,15,"I",1309.4465565502128,"TON",8,{"v":4.509735381340039,"d":"4.51"},{"$f":"VLOOKUP(A45797,cordwood_density!A:D,4,FALSE)","v":1.27},{"v":3.550972741212629,"d":"3.55"}]
["55015","55","WI","015","Calumet","","2104008610","Hydronic heater: outdoor","Hydronic heater",165.91323997774487,"A","CEC Survey",2017,15,"I",650.949697398337,"TON",8,{"v":3.923434305096167,"d":"3.92"},{"$f":"VLOOKUP(A45814,cordwood_density!A:D,4,FALSE)","v":1.3041},{"v":3.008537922779056,"d":"3.01"}]
["55017","55","WI","017","Chippewa","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",479.54055987634996,"A","CEC Survey",2017,15,"I",427.03263255696197,"TON",8,{"v":0.8905036784940001,"d":"0.89"},{"$f":"VLOOKUP(A45835,cordwood_density!A:D,4,FALSE)","v":1.431},{"v":0.622294674,"d":"0.62"}]
["55019","55","WI","019","Clark","","2104009000","Wax Log; Total: All Combustor Types",null,12.422235606954235,"A","CEC Survey",2017,15,"I",6.8446518194317845,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A45853,cordwood_density!A:D,4,FALSE)","v":1.2877},{"v":0.42789469596955815,"d":"0.43"}]
["55025","55","WI","025","Dane","","2104008100","Fireplace: general","Fireplace: general",17452.185319170003,"A","CEC Survey",2017,15,"I",7390.845882142783,"TON",8,{"v":0.42349114148039996,"d":"0.42"},{"$f":"VLOOKUP(A45892,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.325612134,"d":"0.33"}]
["55027","55","WI","027","Dodge","","2104009000","Wax Log; Total: All Combustor Types",null,33.100315293888954,"A","CEC Survey",2017,15,"I",18.238273726932814,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A45913,cordwood_density!A:D,4,FALSE)","v":1.2499},{"v":0.4408352668213457,"d":"0.44"}]
["55029","55","WI","029","Door","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",241.37313311388002,"A","CEC Survey",2017,15,"I",457.76944414369365,"TON",8,{"v":1.8965219460763998,"d":"1.90"},{"$f":"VLOOKUP(A45929,cordwood_density!A:D,4,FALSE)","v":1.1489},{"v":1.6507284759999998,"d":"1.65"}]
["55033","55","WI","033","Dunn","","2104008100","Fireplace: general","Fireplace: general",1185.95394132,"A","CEC Survey",2017,15,"I",677.9122435044968,"TON",8,{"v":0.571617682513,"d":"0.57"},{"$f":"VLOOKUP(A45952,cordwood_density!A:D,4,FALSE)","v":1.381},{"v":0.41391577300000004,"d":"0.41"}]
["55035","55","WI","035","Eau Claire","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",894.7774895811201,"A","CEC Survey",2017,15,"I",820.0380385662572,"TON",8,{"v":0.9164714670573001,"d":"0.92"},{"$f":"VLOOKUP(A45969,cordwood_density!A:D,4,FALSE)","v":1.4107},{"v":0.649657239,"d":"0.65"}]
["55039","55","WI","039","Fond Du Lac","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2286.1250485451296,"A","CEC Survey",2017,15,"I",4076.927163066162,"TON",8,{"v":1.7833351529308004,"d":"1.78"},{"$f":"VLOOKUP(A46005,cordwood_density!A:D,4,FALSE)","v":1.2154},{"v":1.4672825020000002,"d":"1.47"}]
["55041","55","WI","041","Forest","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.02295793834142,"A","CEC Survey",2017,15,"I",62.76142619606573,"TON",8,{"v":4.819291169733971,"d":"4.82"},{"$f":"VLOOKUP(A46008,cordwood_density!A:D,4,FALSE)","v":1.3463},{"v":3.579656220555575,"d":"3.58"}]
["55045","55","WI","045","Green","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",567.515051399,"A","CEC Survey",2017,15,"I",450.57957104715126,"TON",8,{"v":0.793951755,"d":"0.79"},{"$f":"VLOOKUP(A46047,cordwood_density!A:D,4,FALSE)","v":1.3502},{"v":0.5880252962524071,"d":"0.59"}]
["55049","55","WI","049","Iowa","","2104008620","Hydronic heater: indoor","Hydronic heater",103.66948781642947,"A","CEC Survey",2017,15,"I",421.7638603892609,"TON",8,{"v":4.0683509610473845,"d":"4.07"},{"$f":"VLOOKUP(A46070,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.128057020642307,"d":"3.13"}]
["55051","55","WI","051","Iron","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.60558277754779,"A","CEC Survey",2017,15,"I",12.27610424360482,"TON",8,{"v":4.711461999744377,"d":"4.71"},{"$f":"VLOOKUP(A46086,cordwood_density!A:D,4,FALSE)","v":1.3314},{"v":3.538727654907899,"d":"3.54"}]
["55053","55","WI","053","Jackson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",69.25431340512,"A","CEC Survey",2017,15,"I",56.70787972666543,"TON",8,{"v":0.8188353466871999,"d":"0.82"},{"$f":"VLOOKUP(A46103,cordwood_density!A:D,4,FALSE)","v":1.1766},{"v":0.6959334919999999,"d":"0.70"}]
["55055","55","WI","055","Jefferson","","2104009000","Wax Log; Total: All Combustor Types",null,31.88487428742256,"A","CEC Survey",2017,15,"I",17.56856573236983,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46123,cordwood_density!A:D,4,FALSE)","v":1.3706},{"v":0.4020137166204582,"d":"0.40"}]
["55059","55","WI","059","Kenosha","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",328.1120189992155,"A","CEC Survey",2017,15,"I",1218.662178259412,"TON",8,{"v":3.71416500369749,"d":"3.71"},{"$f":"VLOOKUP(A46142,cordwood_density!A:D,4,FALSE)","v":1.395},{"v":2.6624838736182723,"d":"2.66"}]
["55063","55","WI","063","La Crosse","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5466.447979531999,"A","CEC Survey",2017,15,"I",1957.6555852182014,"TON",8,{"v":0.3581220552264,"d":"0.36"},{"$f":"VLOOKUP(A46181,cordwood_density!A:D,4,FALSE)","v":1.1574},{"v":0.309419436,"d":"0.31"}]
["55065","55","WI","065","Lafayette","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",153.30211070832,"A","CEC Survey",2017,15,"I",344.05088600549163,"TON",8,{"v":2.2442671168442,"d":"2.24"},{"$f":"VLOOKUP(A46199,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.725562907,"d":"1.73"}]
["55069","55","WI","069","Lincoln","","2104008620","Hydronic heater: indoor","Hydronic heater",207.47056592048446,"A","CEC Survey",2017,15,"I",909.8098493268105,"TON",8,{"v":4.385247831615334,"d":"4.39"},{"$f":"VLOOKUP(A46220,cordwood_density!A:D,4,FALSE)","v":1.2645},{"v":3.4679698154332415,"d":"3.47"}]
["55071","55","WI","071","Manitowoc","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4578.233995224,"A","CEC Survey",2017,15,"I",1792.0311854410386,"TON",8,{"v":0.3914241140384,"d":"0.39"},{"$f":"VLOOKUP(A46241,cordwood_density!A:D,4,FALSE)","v":1.2704},{"v":0.308110921,"d":"0.31"}]
["55073","55","WI","073","Marathon","","2104009000","Wax Log; Total: All Combustor Types",null,53.38980446673706,"A","CEC Survey",2017,15,"I",29.417782261172125,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46258,cordwood_density!A:D,4,FALSE)","v":1.3451},{"v":0.4096349713775928,"d":"0.41"}]
["55078","55","WI","078","Menominee","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.7820804358934492,"A","CEC Survey",2017,15,"I",9.735491819695305,"TON",8,{"v":5.462992367577616,"d":"5.46"},{"$f":"VLOOKUP(A46296,cordwood_density!A:D,4,FALSE)","v":1.478},{"v":3.696205932055221,"d":"3.70"}]
["55078","55","WI","078","Menominee","","2104008100","Fireplace: general","Fireplace: general",153.859289162,"A","CEC Survey",2017,15,"I",93.23245861160416,"TON",8,{"v":0.605959244446,"d":"0.61"},{"$f":"VLOOKUP(A46297,cordwood_density!A:D,4,FALSE)","v":1.478},{"v":0.409985957,"d":"0.41"}]
["55081","55","WI","081","Monroe","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",975.7686243731999,"A","CEC Survey",2017,15,"I",2400.402837920287,"TON",8,{"v":2.4600123205049997,"d":"2.46"},{"$f":"VLOOKUP(A46336,cordwood_density!A:D,4,FALSE)","v":1.437},{"v":1.7119083649999998,"d":"1.71"}]
["55083","55","WI","083","Oconto","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",395.84441700312,"A","CEC Survey",2017,15,"I",1022.8486354307713,"TON",8,{"v":2.5839663046775,"d":"2.58"},{"$f":"VLOOKUP(A46349,cordwood_density!A:D,4,FALSE)","v":1.3525},{"v":1.9105111309999998,"d":"1.91"}]
["55087","55","WI","087","Outagamie","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",899.3175433436076,"A","CEC Survey",2017,15,"I",650.8752162643892,"TON",8,{"v":0.7237434886953,"d":"0.72"},{"$f":"VLOOKUP(A46375,cordwood_density!A:D,4,FALSE)","v":1.3641},{"v":0.530564833,"d":"0.53"}]
["55089","55","WI","089","Ozaukee","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",964.128320228,"A","CEC Survey",2017,15,"I",632.6778104184918,"TON",8,{"v":0.656217432,"d":"0.66"},{"$f":"VLOOKUP(A46392,cordwood_density!A:D,4,FALSE)","v":1.3267},{"v":0.4946238275420216,"d":"0.49"}]
["55093","55","WI","093","Pierce","","2104008610","Hydronic heater: outdoor","Hydronic heater",220.99590183339637,"A","CEC Survey",2017,15,"I",935.8924280437551,"TON",8,{"v":4.234885897338053,"d":"4.23"},{"$f":"VLOOKUP(A46414,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.256101720235317,"d":"3.26"}]
["55095","55","WI","095","Polk","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",15.000347731981506,"A","CEC Survey",2017,15,"I",69.15358490613983,"TON",8,{"v":4.610132121050825,"d":"4.61"},{"$f":"VLOOKUP(A46431,cordwood_density!A:D,4,FALSE)","v":1.3241},{"v":3.481709932067687,"d":"3.48"}]
["55099","55","WI","099","Price","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",906.7359079191601,"A","CEC Survey",2017,15,"I",2542.2811537660577,"TON",8,{"v":2.803772445276,"d":"2.80"},{"$f":"VLOOKUP(A46470,cordwood_density!A:D,4,FALSE)","v":1.3462},{"v":2.08273098,"d":"2.08"}]
["55103","55","WI","103","Richland","","2104008620","Hydronic heater: indoor","Hydronic heater",82.43771407841975,"A","CEC Survey",2017,15,"I",352.8831719730211,"TON",8,{"v":4.280603555277349,"d":"4.28"},{"$f":"VLOOKUP(A46490,cordwood_density!A:D,4,FALSE)","v":1.333},{"v":3.2112554803280937,"d":"3.21"}]
["55105","55","WI","105","Rock","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1216.0430082537002,"A","CEC Survey",2017,15,"I",777.2925800763373,"TON",8,{"v":0.6391982642066,"d":"0.64"},{"$f":"VLOOKUP(A46509,cordwood_density!A:D,4,FALSE)","v":1.3543},{"v":0.47197686199999994,"d":"0.47"}]
["55107","55","WI","107","Rusk","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",802.776925161,"A","CEC Survey",2017,15,"I",2109.1730285742765,"TON",8,{"v":2.6273463554664,"d":"2.63"},{"$f":"VLOOKUP(A46530,cordwood_density!A:D,4,FALSE)","v":1.3539},{"v":1.9405763759999999,"d":"1.94"}]
["55109","55","WI","109","St Croix","","2104009000","Wax Log; Total: All Combustor Types",null,32.51791647829047,"A","CEC Survey",2017,15,"I",17.917371979538053,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46543,cordwood_density!A:D,4,FALSE)","v":1.3811},{"v":0.398957352834697,"d":"0.40"}]
["55113","55","WI","113","Sawyer","","2104008620","Hydronic heater: indoor","Hydronic heater",195.52141175771882,"A","CEC Survey",2017,15,"I",902.0435584114161,"TON",8,{"v":4.613528259141189,"d":"4.61"},{"$f":"VLOOKUP(A46565,cordwood_density!A:D,4,FALSE)","v":1.2739},{"v":3.6215780352784277,"d":"3.62"}]
["55119","55","WI","119","Taylor","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",23.98342511479885,"A","CEC Survey",2017,15,"I",109.88789292842445,"TON",8,{"v":4.581826507366484,"d":"4.58"},{"$f":"VLOOKUP(A46608,cordwood_density!A:D,4,FALSE)","v":1.2896},{"v":3.5529051701042835,"d":"3.55"}]
["55119","55","WI","119","Taylor","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",252.36267638831998,"A","CEC Survey",2017,15,"I",634.9220939881799,"TON",8,{"v":2.5159112396288004,"d":"2.52"},{"$f":"VLOOKUP(A46619,cordwood_density!A:D,4,FALSE)","v":1.2896},{"v":1.9509237280000002,"d":"1.95"}]
["55121","55","WI","121","Trempealeau","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",528.79716396,"A","CEC Survey",2017,15,"I",764.7361723565188,"TON",8,{"v":1.446180548,"d":"1.45"},{"$f":"VLOOKUP(A46632,cordwood_density!A:D,4,FALSE)","v":1.369},{"v":1.0563773177501827,"d":"1.06"}]
["55121","55","WI","121","Trempealeau","","2104009000","Wax Log; Total: All Combustor Types",null,11.581750359694219,"A","CEC Survey",2017,15,"I",6.381544448191515,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46633,cordwood_density!A:D,4,FALSE)","v":1.369},{"v":0.4024835646457268,"d":"0.40"}]
["55121","55","WI","121","Trempealeau","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",256.35062293631995,"A","CEC Survey",2017,15,"I",648.3036927314138,"TON",8,{"v":2.528972566189,"d":"2.53"},{"$f":"VLOOKUP(A46634,cordwood_density!A:D,4,FALSE)","v":1.369},{"v":1.8473137810000002,"d":"1.85"}]
["55121","55","WI","121","Trempealeau","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1132.2152513020799,"A","CEC Survey",2017,15,"I",2863.3413095637447,"TON",8,{"v":2.528972566189,"d":"2.53"},{"$f":"VLOOKUP(A46635,cordwood_density!A:D,4,FALSE)","v":1.369},{"v":1.8473137810000002,"d":"1.85"}]
["55121","55","WI","121","Trempealeau","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",747.6893168975998,"A","CEC Survey",2017,15,"I",1890.8857704666236,"TON",8,{"v":2.528972566189,"d":"2.53"},{"$f":"VLOOKUP(A46636,cordwood_density!A:D,4,FALSE)","v":1.369},{"v":1.8473137810000002,"d":"1.85"}]
["55123","55","WI","123","Vernon","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",234.27124662387934,"A","CEC Survey",2017,15,"I",985.6219732054964,"TON",8,{"v":4.207182859226019,"d":"4.21"},{"$f":"VLOOKUP(A46637,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.2348015217791932,"d":"3.23"}]
["55123","55","WI","123","Vernon","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",18.994965942476703,"A","CEC Survey",2017,15,"I",79.91529512476997,"TON",8,{"v":4.207182859226018,"d":"4.21"},{"$f":"VLOOKUP(A46638,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.234801521779193,"d":"3.23"}]
["55123","55","WI","123","Vernon","","2104008610","Hydronic heater: outdoor","Hydronic heater",227.9395913097204,"A","CEC Survey",2017,15,"I",958.9835414972397,"TON",8,{"v":4.207182859226019,"d":"4.21"},{"$f":"VLOOKUP(A46639,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.2348015217791932,"d":"3.23"}]
["55123","55","WI","123","Vernon","","2104008620","Hydronic heater: indoor","Hydronic heater",145.62807222565473,"A","CEC Survey",2017,15,"I",612.6839292899032,"TON",8,{"v":4.207182859226018,"d":"4.21"},{"$f":"VLOOKUP(A46640,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.234801521779193,"d":"3.23"}]
["55123","55","WI","123","Vernon","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",6.331655314158901,"A","CEC Survey",2017,15,"I",26.638431708256658,"TON",8,{"v":4.207182859226018,"d":"4.21"},{"$f":"VLOOKUP(A46641,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.234801521779193,"d":"3.23"}]
["55123","55","WI","123","Vernon","","2104008100","Fireplace: general","Fireplace: general",1062.25203502,"A","CEC Survey",2017,15,"I",606.7566726958954,"TON",8,{"v":0.5711984093157999,"d":"0.57"},{"$f":"VLOOKUP(A46642,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.43918069299999996,"d":"0.44"}]
["55123","55","WI","123","Vernon","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",99.322632963,"A","CEC Survey",2017,15,"I",82.68612079967,"TON",8,{"v":0.8325002905478,"d":"0.83"},{"$f":"VLOOKUP(A46643,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.640089413,"d":"0.64"}]
["55123","55","WI","123","Vernon","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",438.67496225325004,"A","CEC Survey",2017,15,"I",365.19703353187583,"TON",8,{"v":0.8325002905478,"d":"0.83"},{"$f":"VLOOKUP(A46644,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.640089413,"d":"0.64"}]
["55123","55","WI","123","Vernon","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",289.69101280875,"A","CEC Survey",2017,15,"I",241.16785233237079,"TON",8,{"v":0.8325002905478,"d":"0.83"},{"$f":"VLOOKUP(A46645,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.640089413,"d":"0.64"}]
["55123","55","WI","123","Vernon","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1969.9816519750002,"A","CEC Survey",2017,15,"I",807.2327764188966,"TON",8,{"v":0.4097666471206,"d":"0.41"},{"$f":"VLOOKUP(A46646,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.315059701,"d":"0.32"}]
["55123","55","WI","123","Vernon","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",554.3902420200001,"A","CEC Survey",2017,15,"I",724.6961374487975,"TON",8,{"v":1.307194973,"d":"1.31"},{"$f":"VLOOKUP(A46647,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.0050707158234662,"d":"1.01"}]
["55123","55","WI","123","Vernon","","2104009000","Wax Log; Total: All Combustor Types",null,11.779454305457584,"A","CEC Survey",2017,15,"I",6.490479322307129,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46648,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.42365062278948185,"d":"0.42"}]
["55123","55","WI","123","Vernon","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",282.0639990612,"A","CEC Survey",2017,15,"I",651.0711101220951,"TON",8,{"v":2.3082389538865997,"d":"2.31"},{"$f":"VLOOKUP(A46649,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.7747493109999999,"d":"1.77"}]
["55123","55","WI","123","Vernon","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1245.7826625203,"A","CEC Survey",2017,15,"I",2875.5640697059202,"TON",8,{"v":2.3082389538865997,"d":"2.31"},{"$f":"VLOOKUP(A46650,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.7747493109999999,"d":"1.77"}]
["55123","55","WI","123","Vernon","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",822.6866639284999,"A","CEC Survey",2017,15,"I",1898.9574045227773,"TON",8,{"v":2.3082389538865997,"d":"2.31"},{"$f":"VLOOKUP(A46651,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.7747493109999999,"d":"1.77"}]
["55125","55","WI","125","Vilas","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",446.6758016228913,"A","CEC Survey",2017,15,"I",1874.652992458098,"TON",8,{"v":4.1968984790467445,"d":"4.20"},{"$f":"VLOOKUP(A46652,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":3.5217743383794113,"d":"3.52"}]
["55125","55","WI","125","Vilas","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",36.21695688834254,"A","CEC Survey",2017,15,"I",151.99889128038632,"TON",8,{"v":4.1968984790467445,"d":"4.20"},{"$f":"VLOOKUP(A46653,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":3.5217743383794113,"d":"3.52"}]
["55125","55","WI","125","Vilas","","2104008610","Hydronic heater: outdoor","Hydronic heater",434.60348266011044,"A","CEC Survey",2017,15,"I",1823.9866953646358,"TON",8,{"v":4.1968984790467445,"d":"4.20"},{"$f":"VLOOKUP(A46654,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":3.5217743383794113,"d":"3.52"}]
["55125","55","WI","125","Vilas","","2104008620","Hydronic heater: indoor","Hydronic heater",277.6633361439595,"A","CEC Survey",2017,15,"I",1165.3248331496286,"TON",8,{"v":4.1968984790467445,"d":"4.20"},{"$f":"VLOOKUP(A46655,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":3.5217743383794113,"d":"3.52"}]
["55125","55","WI","125","Vilas","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",12.072318962780846,"A","CEC Survey",2017,15,"I",50.666297093462106,"TON",8,{"v":4.1968984790467445,"d":"4.20"},{"$f":"VLOOKUP(A46656,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":3.5217743383794113,"d":"3.52"}]
["55125","55","WI","125","Vilas","","2104008100","Fireplace: general","Fireplace: general",1516.594010316,"A","CEC Survey",2017,15,"I",758.8205539913002,"TON",8,{"v":0.5003452135705001,"d":"0.50"},{"$f":"VLOOKUP(A46657,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":0.41985836500000007,"d":"0.42"}]
["55125","55","WI","125","Vilas","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",97.49664407736,"A","CEC Survey",2017,15,"I",99.73612826992478,"TON",8,{"v":1.0229698592578,"d":"1.02"},{"$f":"VLOOKUP(A46658,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":0.858412234,"d":"0.86"}]
["55125","55","WI","125","Vilas","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",430.61017800834003,"A","CEC Survey",2017,15,"I",440.5012331921678,"TON",8,{"$f":"P46659/J46659","v":{"v":1.0229698592578,"d":"1.02"}},{"$f":"VLOOKUP(A46659,cordwood_density!A:D,4,FALSE)","v":1.1917},{"$f":"S46659/T46659","v":{"v":0.858412234,"d":"0.86"}}]
["55125","55","WI","125","Vilas","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",284.3652118923,"A","CEC Survey",2017,15,"I",290.89704078728056,"TON",8,{"v":1.0229698592577998,"d":"1.02"},{"$f":"VLOOKUP(A46660,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":0.8584122339999999,"d":"0.86"}]
["55125","55","WI","125","Vilas","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1983.05796414,"A","CEC Survey",2017,15,"I",742.7884078755905,"TON",8,{"v":0.3745671691436,"d":"0.37"},{"$f":"VLOOKUP(A46661,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":0.314313308,"d":"0.31"}]
["55125","55","WI","125","Vilas","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",577.474895184,"A","CEC Survey",2017,15,"I",1533.646148354862,"TON",8,{"v":2.655779777,"d":"2.66"},{"$f":"VLOOKUP(A46662,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":2.2285640488377947,"d":"2.23"}]
["55125","55","WI","125","Vilas","","2104009000","Wax Log; Total: All Combustor Types",null,10.477335214395426,"A","CEC Survey",2017,15,"I",5.77301170313188,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46663,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":0.46236468909960565,"d":"0.46"}]
["55125","55","WI","125","Vilas","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",328.82466240360003,"A","CEC Survey",2017,15,"I",799.9967128886342,"TON",8,{"v":2.4328975419329,"d":"2.43"},{"$f":"VLOOKUP(A46664,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":2.041535237,"d":"2.04"}]
["55125","55","WI","125","Vilas","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1452.3089256159,"A","CEC Survey",2017,15,"I",3533.3188152581347,"TON",8,{"v":2.4328975419329004,"d":"2.43"},{"$f":"VLOOKUP(A46665,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":2.041535237,"d":"2.04"}]
["55125","55","WI","125","Vilas","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",959.0719320105,"A","CEC Survey",2017,15,"I",2333.323745925183,"TON",8,{"v":2.4328975419329004,"d":"2.43"},{"$f":"VLOOKUP(A46666,cordwood_density!A:D,4,FALSE)","v":1.1917},{"v":2.041535237,"d":"2.04"}]
["55127","55","WI","127","Walworth","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",301.8761908241693,"A","CEC Survey",2017,15,"I",1246.1098864786456,"TON",8,{"v":4.1278839615557965,"d":"4.13"},{"$f":"VLOOKUP(A46667,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":2.928408031750707,"d":"2.93"}]
["55127","55","WI","127","Walworth","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",24.476447904662376,"A","CEC Survey",2017,15,"I",101.0359367415118,"TON",8,{"v":4.1278839615557965,"d":"4.13"},{"$f":"VLOOKUP(A46668,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":2.928408031750707,"d":"2.93"}]
["55127","55","WI","127","Walworth","","2104008610","Hydronic heater: outdoor","Hydronic heater",293.7173748559485,"A","CEC Survey",2017,15,"I",1212.4312408981416,"TON",8,{"v":4.1278839615557965,"d":"4.13"},{"$f":"VLOOKUP(A46669,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":2.928408031750707,"d":"2.93"}]
["55127","55","WI","127","Walworth","","2104008620","Hydronic heater: indoor","Hydronic heater",187.65276726907823,"A","CEC Survey",2017,15,"I",774.6088483515905,"TON",8,{"v":4.1278839615557965,"d":"4.13"},{"$f":"VLOOKUP(A46670,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":2.928408031750707,"d":"2.93"}]
["55127","55","WI","127","Walworth","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",8.158815968220793,"A","CEC Survey",2017,15,"I",33.67864558050393,"TON",8,{"v":4.127883961555796,"d":"4.13"},{"$f":"VLOOKUP(A46671,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":2.928408031750706,"d":"2.93"}]
["55127","55","WI","127","Walworth","","2104008100","Fireplace: general","Fireplace: general",4139.878147148,"A","CEC Survey",2017,15,"I",2279.408583538177,"TON",8,{"v":0.5505979892448001,"d":"0.55"},{"$f":"VLOOKUP(A46672,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.39060583800000004,"d":"0.39"}]
["55127","55","WI","127","Walworth","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",168.62559334152,"A","CEC Survey",2017,15,"I",120.79283690109433,"TON",8,{"v":0.7163375055199999,"d":"0.72"},{"$f":"VLOOKUP(A46673,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.50818495,"d":"0.51"}]
["55127","55","WI","127","Walworth","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",744.76303725838,"A","CEC Survey",2017,15,"I",533.5016963131667,"TON",8,{"v":0.71633750552,"d":"0.72"},{"$f":"VLOOKUP(A46674,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.50818495,"d":"0.51"}]
["55127","55","WI","127","Walworth","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",491.82464724609997,"A","CEC Survey",2017,15,"I",352.3124409615251,"TON",8,{"v":0.7163375055199999,"d":"0.72"},{"$f":"VLOOKUP(A46675,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.50818495,"d":"0.51"}]
["55127","55","WI","127","Walworth","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,5145.0817222119995,"A","CEC Survey",2017,15,"I",2266.4008109767583,"TON",8,{"v":0.44049850582399996,"d":"0.44"},{"$f":"VLOOKUP(A46676,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.31249894,"d":"0.31"}]
["55127","55","WI","127","Walworth","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1224.62581346,"A","CEC Survey",2017,15,"I",794.0538973552948,"TON",8,{"v":0.648405324,"d":"0.65"},{"$f":"VLOOKUP(A46677,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.4599924262202043,"d":"0.46"}]
["55127","55","WI","127","Walworth","","2104009000","Wax Log; Total: All Combustor Types",null,39.19602463641554,"A","CEC Survey",2017,15,"I",21.597009574664963,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46678,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":0.39089103291713967,"d":"0.39"}]
["55127","55","WI","127","Walworth","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",430.35393915599997,"A","CEC Survey",2017,15,"I",876.2208409438795,"TON",8,{"v":2.0360469864927997,"d":"2.04"},{"$f":"VLOOKUP(A46679,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":1.4444147179999998,"d":"1.44"}]
["55127","55","WI","127","Walworth","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1900.729897939,"A","CEC Survey",2017,15,"I",3869.975380835468,"TON",8,{"v":2.0360469864927997,"d":"2.04"},{"$f":"VLOOKUP(A46680,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":1.4444147179999998,"d":"1.44"}]
["55127","55","WI","127","Walworth","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1255.1989892049999,"A","CEC Survey",2017,15,"I",2555.644119419648,"TON",8,{"v":2.0360469864927997,"d":"2.04"},{"$f":"VLOOKUP(A46681,cordwood_density!A:D,4,FALSE)","v":1.4096},{"v":1.4444147179999998,"d":"1.44"}]
["55129","55","WI","129","Washburn","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",266.8279436213269,"A","CEC Survey",2017,15,"I",1250.9134087641223,"TON",8,{"v":4.688089979583907,"d":"4.69"},{"$f":"VLOOKUP(A46682,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":3.5716059573243237,"d":"3.57"}]
["55129","55","WI","129","Washburn","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",21.634698131458936,"A","CEC Survey",2017,15,"I",101.42541152141531,"TON",8,{"v":4.688089979583907,"d":"4.69"},{"$f":"VLOOKUP(A46683,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":3.5716059573243237,"d":"3.57"}]
["55129","55","WI","129","Washburn","","2104008610","Hydronic heater: outdoor","Hydronic heater",259.61637757750725,"A","CEC Survey",2017,15,"I",1217.1049382569838,"TON",8,{"v":4.688089979583907,"d":"4.69"},{"$f":"VLOOKUP(A46684,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":3.5716059573243237,"d":"3.57"}]
["55129","55","WI","129","Washburn","","2104008620","Hydronic heater: indoor","Hydronic heater",165.86601900785186,"A","CEC Survey",2017,15,"I",777.5948216641841,"TON",8,{"v":4.688089979583907,"d":"4.69"},{"$f":"VLOOKUP(A46685,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":3.5716059573243237,"d":"3.57"}]
["55129","55","WI","129","Washburn","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",7.211566043819646,"A","CEC Survey",2017,15,"I",33.80847050713844,"TON",8,{"v":4.688089979583906,"d":"4.69"},{"$f":"VLOOKUP(A46686,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":3.571605957324323,"d":"3.57"}]
["55129","55","WI","129","Washburn","","2104008100","Fireplace: general","Fireplace: general",813.748574166,"A","CEC Survey",2017,15,"I",437.42265106940243,"TON",8,{"v":0.5375402980185999,"d":"0.54"},{"$f":"VLOOKUP(A46687,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":0.40952331099999995,"d":"0.41"}]
["55129","55","WI","129","Washburn","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",71.53203712535999,"A","CEC Survey",2017,15,"I",76.38343708591258,"TON",8,{"v":1.0678213588696,"d":"1.07"},{"$f":"VLOOKUP(A46688,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":0.8135161959999999,"d":"0.81"}]
["55129","55","WI","129","Washburn","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",315.93316397034,"A","CEC Survey",2017,15,"I",337.3601804627806,"TON",8,{"v":1.0678213588696,"d":"1.07"},{"$f":"VLOOKUP(A46689,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":0.8135161959999999,"d":"0.81"}]
["55129","55","WI","129","Washburn","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",208.63510828229997,"A","CEC Survey",2017,15,"I",222.78502483391168,"TON",8,{"v":1.0678213588696,"d":"1.07"},{"$f":"VLOOKUP(A46690,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":0.8135161959999999,"d":"0.81"}]
["55129","55","WI","129","Washburn","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1270.4996646,"A","CEC Survey",2017,15,"I",525.6787169843883,"TON",8,{"v":0.4137574622264,"d":"0.41"},{"$f":"VLOOKUP(A46691,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":0.31521976399999996,"d":"0.32"}]
["55129","55","WI","129","Washburn","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",354.70817991,"A","CEC Survey",2017,15,"I",931.0691885489995,"TON",8,{"v":2.624887841,"d":"2.62"},{"$f":"VLOOKUP(A46692,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":1.9997621826908427,"d":"2.00"}]
["55129","55","WI","129","Washburn","","2104009000","Wax Log; Total: All Combustor Types",null,6.955672811044073,"A","CEC Survey",2017,15,"I",3.8325757188852845,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46693,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":0.41977754075879936,"d":"0.42"}]
["55129","55","WI","129","Washburn","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",221.73375818423997,"A","CEC Survey",2017,15,"I",569.8402726833912,"TON",8,{"v":2.5699301601603994,"d":"2.57"},{"$f":"VLOOKUP(A46694,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":1.9578928539999996,"d":"1.96"}]
["55129","55","WI","129","Washburn","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",979.3240986470599,"A","CEC Survey",2017,15,"I",2516.794537684978,"TON",8,{"v":2.5699301601604,"d":"2.57"},{"$f":"VLOOKUP(A46695,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":1.957892854,"d":"1.96"}]
["55129","55","WI","129","Washburn","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",646.7234613706999,"A","CEC Survey",2017,15,"I",1662.034128659891,"TON",8,{"v":2.5699301601604,"d":"2.57"},{"$f":"VLOOKUP(A46696,cordwood_density!A:D,4,FALSE)","v":1.3126},{"v":1.957892854,"d":"1.96"}]
["55131","55","WI","131","Washington","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",396.3777314333772,"A","CEC Survey",2017,15,"I",1571.874612190004,"TON",8,{"v":3.9655976800356734,"d":"3.97"},{"$f":"VLOOKUP(A46697,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":2.9223269565480274,"d":"2.92"}]
["55131","55","WI","131","Washington","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",32.13873498108464,"A","CEC Survey",2017,15,"I",127.44929288027058,"TON",8,{"v":3.965597680035673,"d":"3.97"},{"$f":"VLOOKUP(A46698,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":2.9223269565480274,"d":"2.92"}]
["55131","55","WI","131","Washington","","2104008610","Hydronic heater: outdoor","Hydronic heater",385.66481977301567,"A","CEC Survey",2017,15,"I",1529.391514563247,"TON",8,{"v":3.9655976800356734,"d":"3.97"},{"$f":"VLOOKUP(A46699,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":2.9223269565480274,"d":"2.92"}]
["55131","55","WI","131","Washington","","2104008620","Hydronic heater: indoor","Hydronic heater",246.39696818831558,"A","CEC Survey",2017,15,"I",977.1112454154079,"TON",8,{"v":3.9655976800356734,"d":"3.97"},{"$f":"VLOOKUP(A46700,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":2.9223269565480274,"d":"2.92"}]
["55131","55","WI","131","Washington","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.712911660361547,"A","CEC Survey",2017,15,"I",42.483097626756866,"TON",8,{"v":3.9655976800356734,"d":"3.97"},{"$f":"VLOOKUP(A46701,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":2.9223269565480274,"d":"2.92"}]
["55131","55","WI","131","Washington","","2104008100","Fireplace: general","Fireplace: general",5761.543943556,"A","CEC Survey",2017,15,"I",2903.783108693923,"TON",8,{"v":0.503993918495,"d":"0.50"},{"$f":"VLOOKUP(A46702,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.371403035,"d":"0.37"}]
["55131","55","WI","131","Washington","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",229.0077202992,"A","CEC Survey",2017,15,"I",168.55917616456938,"TON",8,{"v":0.736041457224,"d":"0.74"},{"$f":"VLOOKUP(A46703,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.5424034320000001,"d":"0.54"}]
["55131","55","WI","131","Washington","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1011.4507646548001,"A","CEC Survey",2017,15,"I",744.4696947268482,"TON",8,{"v":0.736041457224,"d":"0.74"},{"$f":"VLOOKUP(A46704,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.5424034320000001,"d":"0.54"}]
["55131","55","WI","131","Washington","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",667.9391842059999,"A","CEC Survey",2017,15,"I",491.630930479994,"TON",8,{"v":0.736041457224,"d":"0.74"},{"$f":"VLOOKUP(A46705,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.5424034320000001,"d":"0.54"}]
["55131","55","WI","131","Washington","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,6754.287604083999,"A","CEC Survey",2017,15,"I",2871.1392119927823,"TON",8,{"v":0.42508394375400005,"d":"0.43"},{"$f":"VLOOKUP(A46706,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.31325272200000004,"d":"0.31"}]
["55131","55","WI","131","Washington","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1543.788299372,"A","CEC Survey",2017,15,"I",1121.744496191301,"TON",8,{"v":0.726618084,"d":"0.73"},{"$f":"VLOOKUP(A46707,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.5354591628592484,"d":"0.54"}]
["55131","55","WI","131","Washington","","2104009000","Wax Log; Total: All Combustor Types",null,1025.864414919135,"A","CEC Survey",2017,15,"I",572.3290343516464,"TON",8,{"v":0.55789929549,"d":"0.56"},{"$f":"VLOOKUP(A46708,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":0.4111269679366249,"d":"0.41"}]
["55131","55","WI","131","Washington","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",565.7706800476799,"A","CEC Survey",2017,15,"I",1073.6300218415258,"TON",8,{"v":1.8976416765730004,"d":"1.90"},{"$f":"VLOOKUP(A46709,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":1.3984094890000003,"d":"1.40"}]
["55131","55","WI","131","Washington","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2498.82050354392,"A","CEC Survey",2017,15,"I",4741.865929800073,"TON",8,{"v":1.8976416765730002,"d":"1.90"},{"$f":"VLOOKUP(A46710,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":1.398409489,"d":"1.40"}]
["55131","55","WI","131","Washington","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1650.1644834723998,"A","CEC Survey",2017,15,"I",3131.4208970377836,"TON",8,{"v":1.8976416765730002,"d":"1.90"},{"$f":"VLOOKUP(A46711,cordwood_density!A:D,4,FALSE)","v":1.357},{"v":1.398409489,"d":"1.40"}]
["55133","55","WI","133","Waukesha","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",875.4822750354364,"A","CEC Survey",2017,15,"I",2850.885524039753,"TON",8,{"v":3.2563600718522365,"d":"3.26"},{"$f":"VLOOKUP(A46712,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":2.6326785284600502,"d":"2.63"}]
["55133","55","WI","133","Waukesha","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",70.98504932719754,"A","CEC Survey",2017,15,"I",231.1528803275475,"TON",8,{"v":3.256360071852236,"d":"3.26"},{"$f":"VLOOKUP(A46713,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":2.63267852846005,"d":"2.63"}]
["55133","55","WI","133","Waukesha","","2104008610","Hydronic heater: outdoor","Hydronic heater",851.8205919263705,"A","CEC Survey",2017,15,"I",2773.8345639305703,"TON",8,{"v":3.256360071852236,"d":"3.26"},{"$f":"VLOOKUP(A46714,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":2.63267852846005,"d":"2.63"}]
["55133","55","WI","133","Waukesha","","2104008620","Hydronic heater: indoor","Hydronic heater",544.2187115085145,"A","CEC Survey",2017,15,"I",1772.1720825111977,"TON",8,{"v":3.256360071852236,"d":"3.26"},{"$f":"VLOOKUP(A46715,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":2.63267852846005,"d":"2.63"}]
["55133","55","WI","133","Waukesha","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",23.661683109065848,"A","CEC Survey",2017,15,"I",77.05096010918251,"TON",8,{"v":3.2563600718522365,"d":"3.26"},{"$f":"VLOOKUP(A46716,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":2.6326785284600502,"d":"2.63"}]
["55133","55","WI","133","Waukesha","","2104008100","Fireplace: general","Fireplace: general",19871.967927923997,"A","CEC Survey",2017,15,"I",7408.991377008849,"TON",8,{"v":0.37283631917490007,"d":"0.37"},{"$f":"VLOOKUP(A46717,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.30142802100000005,"d":"0.30"}]
["55133","55","WI","133","Waukesha","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",627.32915084448,"A","CEC Survey",2017,15,"I",429.89445618320593,"TON",8,{"v":0.6852773469948,"d":"0.69"},{"$f":"VLOOKUP(A46718,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.554028092,"d":"0.55"}]
["55133","55","WI","133","Waukesha","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2770.70374956312,"A","CEC Survey",2017,15,"I",1898.7005148091596,"TON",8,{"v":0.6852773469948,"d":"0.69"},{"$f":"VLOOKUP(A46719,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.554028092,"d":"0.55"}]
["55133","55","WI","133","Waukesha","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",1829.7100232963996,"A","CEC Survey",2017,15,"I",1253.8588305343505,"TON",8,{"v":0.6852773469948,"d":"0.69"},{"$f":"VLOOKUP(A46720,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.554028092,"d":"0.55"}]
["55133","55","WI","133","Waukesha","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,17507.6169597,"A","CEC Survey",2017,15,"I",7472.256963240862,"TON",8,{"v":0.4268003452692,"d":"0.43"},{"$f":"VLOOKUP(A46721,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.345056468,"d":"0.35"}]
["55133","55","WI","133","Waukesha","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",3934.435309056,"A","CEC Survey",2017,15,"I",3010.600834816023,"TON",8,{"v":0.765192613,"d":"0.77"},{"$f":"VLOOKUP(A46722,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":0.6186374104616379,"d":"0.62"}]
["55133","55","WI","133","Waukesha","","2104009000","Wax Log; Total: All Combustor Types",null,2996.067595889659,"A","CEC Survey",2017,15,"I",1671.5040009872587,"TON",8,{"$f":"P46723/J46723","v":{"v":0.55789929549,"d":"0.56"}},{"$f":"VLOOKUP(A46723,cordwood_density!A:D,4,FALSE)","v":1.2369},{"$f":"S46723/T46723","v":{"v":0.4510464026922143,"d":"0.45"}}]
["55133","55","WI","133","Waukesha","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",1351.18757488176,"A","CEC Survey",2017,15,"I",2022.667762147929,"TON",8,{"v":1.4969555669019003,"d":"1.50"},{"$f":"VLOOKUP(A46724,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":1.210247851,"d":"1.21"}]
["55133","55","WI","133","Waukesha","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",5967.74512239444,"A","CEC Survey",2017,15,"I",8933.44928282002,"TON",8,{"v":1.4969555669019003,"d":"1.50"},{"$f":"VLOOKUP(A46725,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":1.210247851,"d":"1.21"}]
["55133","55","WI","133","Waukesha","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",3940.9637600717992,"A","CEC Survey",2017,15,"I",5899.4476395981255,"TON",8,{"v":1.4969555669019006,"d":"1.50"},{"$f":"VLOOKUP(A46726,cordwood_density!A:D,4,FALSE)","v":1.2369},{"v":1.2102478510000003,"d":"1.21"}]
["55135","55","WI","135","Waupaca","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",382.5436765303985,"A","CEC Survey",2017,15,"I",1584.9585677554812,"TON",8,{"v":4.143209429393179,"d":"4.14"},{"$f":"VLOOKUP(A46727,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":3.240173167586752,"d":"3.24"}]
["55135","55","WI","135","Waupaca","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",31.017054853816095,"A","CEC Survey",2017,15,"I",128.51015414233632,"TON",8,{"v":4.143209429393179,"d":"4.14"},{"$f":"VLOOKUP(A46728,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":3.240173167586752,"d":"3.24"}]
["55135","55","WI","135","Waupaca","","2104008610","Hydronic heater: outdoor","Hydronic heater",372.20465824579315,"A","CEC Survey",2017,15,"I",1542.1218497080358,"TON",8,{"v":4.1432094293931785,"d":"4.14"},{"$f":"VLOOKUP(A46729,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":3.240173167586751,"d":"3.24"}]
["55135","55","WI","135","Waupaca","","2104008620","Hydronic heater: indoor","Hydronic heater",237.79742054592342,"A","CEC Survey",2017,15,"I",985.2445150912451,"TON",8,{"v":4.1432094293931785,"d":"4.14"},{"$f":"VLOOKUP(A46730,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":3.240173167586751,"d":"3.24"}]
["55135","55","WI","135","Waupaca","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.339018284605366,"A","CEC Survey",2017,15,"I",42.83671804744544,"TON",8,{"v":4.1432094293931785,"d":"4.14"},{"$f":"VLOOKUP(A46731,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":3.240173167586751,"d":"3.24"}]
["55135","55","WI","135","Waupaca","","2104008100","Fireplace: general","Fireplace: general",2421.485238519,"A","CEC Survey",2017,15,"I",1244.1158480661093,"TON",8,{"v":0.5137821318403,"d":"0.51"},{"$f":"VLOOKUP(A46732,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":0.401800369,"d":"0.40"}]
["55135","55","WI","135","Waupaca","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",150.41771897051999,"A","CEC Survey",2017,15,"I",132.39961753341518,"TON",8,{"v":0.8802129060298001,"d":"0.88"},{"$f":"VLOOKUP(A46733,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":0.688365454,"d":"0.69"}]
["55135","55","WI","135","Waupaca","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",664.34492545313,"A","CEC Survey",2017,15,"I",584.7649774392505,"TON",8,{"v":0.8802129060298002,"d":"0.88"},{"$f":"VLOOKUP(A46734,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":0.6883654540000002,"d":"0.69"}]
["55135","55","WI","135","Waupaca","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",438.71834699734995,"A","CEC Survey",2017,15,"I",386.1655511391276,"TON",8,{"v":0.8802129060298001,"d":"0.88"},{"$f":"VLOOKUP(A46735,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":0.688365454,"d":"0.69"}]
["55135","55","WI","135","Waupaca","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3307.916167309,"A","CEC Survey",2017,15,"I",1326.4161901317793,"TON",8,{"v":0.4009824079704,"d":"0.40"},{"$f":"VLOOKUP(A46736,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":0.31358599200000004,"d":"0.31"}]
["55135","55","WI","135","Waupaca","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",864.266162003,"A","CEC Survey",2017,15,"I",1179.5525278191524,"TON",8,{"v":1.3648023950000001,"d":"1.36"},{"$f":"VLOOKUP(A46737,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":1.0673358841010403,"d":"1.07"}]
["55135","55","WI","135","Waupaca","","2104009000","Wax Log; Total: All Combustor Types",null,21.224443793206873,"A","CEC Survey",2017,15,"I",11.694668530056989,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46738,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":0.43090638930163455,"d":"0.43"}]
["55135","55","WI","135","Waupaca","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",420.42383852567997,"A","CEC Survey",2017,15,"I",932.0572743886686,"TON",8,{"v":2.2169467784157,"d":"2.22"},{"$f":"VLOOKUP(A46739,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":1.733750511,"d":"1.73"}]
["55135","55","WI","135","Waupaca","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1856.87195348842,"A","CEC Survey",2017,15,"I",4116.58629521662,"TON",8,{"v":2.2169467784156995,"d":"2.22"},{"$f":"VLOOKUP(A46740,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":1.7337505109999998,"d":"1.73"}]
["55135","55","WI","135","Waupaca","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1226.2361956999,"A","CEC Survey",2017,15,"I",2718.5003836336164,"TON",8,{"v":2.2169467784156995,"d":"2.22"},{"$f":"VLOOKUP(A46741,cordwood_density!A:D,4,FALSE)","v":1.2787},{"v":1.7337505109999998,"d":"1.73"}]
["55137","55","WI","137","Waushara","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",223.24223930779277,"A","CEC Survey",2017,15,"I",1034.648451223222,"TON",8,{"v":4.6346446552021545,"d":"4.63"},{"$f":"VLOOKUP(A46742,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":3.299149099659848,"d":"3.30"}]
["55137","55","WI","137","Waushara","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",18.10072210603725,"A","CEC Survey",2017,15,"I",83.89041496404502,"TON",8,{"v":4.6346446552021545,"d":"4.63"},{"$f":"VLOOKUP(A46743,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":3.299149099659848,"d":"3.30"}]
["55137","55","WI","137","Waushara","","2104008610","Hydronic heater: outdoor","Hydronic heater",217.208665272447,"A","CEC Survey",2017,15,"I",1006.6849795685403,"TON",8,{"v":4.6346446552021545,"d":"4.63"},{"$f":"VLOOKUP(A46744,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":3.299149099659848,"d":"3.30"}]
["55137","55","WI","137","Waushara","","2104008620","Hydronic heater: indoor","Hydronic heater",138.77220281295226,"A","CEC Survey",2017,15,"I",643.1598480576786,"TON",8,{"v":4.6346446552021545,"d":"4.63"},{"$f":"VLOOKUP(A46745,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":3.299149099659848,"d":"3.30"}]
["55137","55","WI","137","Waushara","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",6.033574035345751,"A","CEC Survey",2017,15,"I",27.963471654681676,"TON",8,{"v":4.634644655202154,"d":"4.63"},{"$f":"VLOOKUP(A46746,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":3.2991490996598474,"d":"3.30"}]
["55137","55","WI","137","Waushara","","2104008100","Fireplace: general","Fireplace: general",847.907053796,"A","CEC Survey",2017,15,"I",528.6467000189067,"TON",8,{"v":0.6234724639360001,"d":"0.62"},{"$f":"VLOOKUP(A46747,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":0.44381582,"d":"0.44"}]
["55137","55","WI","137","Waushara","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",79.27097296355998,"A","CEC Survey",2017,15,"I",68.05226116947195,"TON",8,{"v":0.8584764211328003,"d":"0.86"},{"$f":"VLOOKUP(A46748,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":0.6111022360000002,"d":"0.61"}]
["55137","55","WI","137","Waushara","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",350.11346392239,"A","CEC Survey",2017,15,"I",300.5641534985011,"TON",8,{"v":0.8584764211328002,"d":"0.86"},{"$f":"VLOOKUP(A46749,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":0.6111022360000001,"d":"0.61"}]
["55137","55","WI","137","Waushara","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",231.20700447704996,"A","CEC Survey",2017,15,"I",198.48576174429317,"TON",8,{"v":0.8584764211328002,"d":"0.86"},{"$f":"VLOOKUP(A46750,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":0.6111022360000001,"d":"0.61"}]
["55137","55","WI","137","Waushara","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1631.757536797,"A","CEC Survey",2017,15,"I",723.1558969873772,"TON",8,{"v":0.4431760728416001,"d":"0.44"},{"$f":"VLOOKUP(A46751,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":0.31547271700000007,"d":"0.32"}]
["55137","55","WI","137","Waushara","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",472.302087133,"A","CEC Survey",2017,15,"I",675.715592765835,"TON",8,{"v":1.430685172,"d":"1.43"},{"$f":"VLOOKUP(A46752,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":1.0184262329157174,"d":"1.02"}]
["55137","55","WI","137","Waushara","","2104009000","Wax Log; Total: All Combustor Types",null,9.593997880368967,"A","CEC Survey",2017,15,"I",5.286292832083301,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46753,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":0.39222665148063784,"d":"0.39"}]
["55137","55","WI","137","Waushara","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",245.21012581392,"A","CEC Survey",2017,15,"I",625.2942964048177,"TON",8,{"v":2.5500345645568,"d":"2.55"},{"$f":"VLOOKUP(A46754,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":1.815229616,"d":"1.82"}]
["55137","55","WI","137","Waushara","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1083.01138901148,"A","CEC Survey",2017,15,"I",2761.716475787945,"TON",8,{"v":2.5500345645568,"d":"2.55"},{"$f":"VLOOKUP(A46755,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":1.815229616,"d":"1.82"}]
["55137","55","WI","137","Waushara","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",715.1962002906,"A","CEC Survey",2017,15,"I",1823.7750311807183,"TON",8,{"v":2.5500345645568,"d":"2.55"},{"$f":"VLOOKUP(A46756,cordwood_density!A:D,4,FALSE)","v":1.4048},{"v":1.815229616,"d":"1.82"}]
["55139","55","WI","139","Winnebago","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",421.1180054351843,"A","CEC Survey",2017,15,"I",1532.5399014651798,"TON",8,{"v":3.639217230527699,"d":"3.64"},{"$f":"VLOOKUP(A46757,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":2.859670933936586,"d":"2.86"}]
["55139","55","WI","139","Winnebago","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",34.14470314339332,"A","CEC Survey",2017,15,"I",124.25999201069024,"TON",8,{"v":3.639217230527698,"d":"3.64"},{"$f":"VLOOKUP(A46758,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":2.8596709339365853,"d":"2.86"}]
["55139","55","WI","139","Winnebago","","2104008610","Hydronic heater: outdoor","Hydronic heater",409.73643772071983,"A","CEC Survey",2017,15,"I",1491.119904128283,"TON",8,{"v":3.6392172305276986,"d":"3.64"},{"$f":"VLOOKUP(A46759,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":2.8596709339365853,"d":"2.86"}]
["55139","55","WI","139","Winnebago","","2104008620","Hydronic heater: indoor","Hydronic heater",261.77605743268214,"A","CEC Survey",2017,15,"I",952.6599387486252,"TON",8,{"v":3.6392172305276986,"d":"3.64"},{"$f":"VLOOKUP(A46760,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":2.8596709339365853,"d":"2.86"}]
["55139","55","WI","139","Winnebago","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",11.38156771446444,"A","CEC Survey",2017,15,"I",41.41999733689675,"TON",8,{"v":3.6392172305276986,"d":"3.64"},{"$f":"VLOOKUP(A46761,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":2.8596709339365853,"d":"2.86"}]
["55139","55","WI","139","Winnebago","","2104008100","Fireplace: general","Fireplace: general",6150.148695441,"A","CEC Survey",2017,15,"I",2657.864472884605,"TON",8,{"v":0.43216263614160005,"d":"0.43"},{"$f":"VLOOKUP(A46762,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.33959031600000006,"d":"0.34"}]
["55139","55","WI","139","Winnebago","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",260.75970286236,"A","CEC Survey",2017,15,"I",153.52656403904055,"TON",8,{"v":0.5887664480124001,"d":"0.59"},{"$f":"VLOOKUP(A46763,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.4626484740000001,"d":"0.46"}]
["55139","55","WI","139","Winnebago","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1151.6886876420901,"A","CEC Survey",2017,15,"I",678.0756578390958,"TON",8,{"v":0.5887664480124,"d":"0.59"},{"$f":"VLOOKUP(A46764,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.462648474,"d":"0.46"}]
["55139","55","WI","139","Winnebago","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",760.54913334855,"A","CEC Survey",2017,15,"I",447.7858117805349,"TON",8,{"v":0.5887664480124,"d":"0.59"},{"$f":"VLOOKUP(A46765,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.462648474,"d":"0.46"}]
["55139","55","WI","139","Winnebago","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,7868.0708714699995,"A","CEC Survey",2017,15,"I",3160.7907009364158,"TON",8,{"v":0.40172372015580005,"d":"0.40"},{"$f":"VLOOKUP(A46766,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.31567163300000006,"d":"0.32"}]
["55139","55","WI","139","Winnebago","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1740.6998847090001,"A","CEC Survey",2017,15,"I",1161.4585821772312,"TON",8,{"v":0.667236548,"d":"0.67"},{"$f":"VLOOKUP(A46767,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.5243097186861544,"d":"0.52"}]
["55139","55","WI","139","Winnebago","","2104009000","Wax Log; Total: All Combustor Types",null,67.9390618350075,"A","CEC Survey",2017,15,"I",37.434423071089135,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46768,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":0.432971868615433,"d":"0.43"}]
["55139","55","WI","139","Winnebago","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",640.52814531996,"A","CEC Survey",2017,15,"I",1059.9629076953531,"TON",8,{"v":1.6548264357155997,"d":"1.65"},{"$f":"VLOOKUP(A46769,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":1.3003508059999997,"d":"1.30"}]
["55139","55","WI","139","Winnebago","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2828.9993084964904,"A","CEC Survey",2017,15,"I",4681.502842321143,"TON",8,{"v":1.6548264357155997,"d":"1.65"},{"$f":"VLOOKUP(A46770,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":1.3003508059999997,"d":"1.30"}]
["55139","55","WI","139","Winnebago","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1868.2070905165501,"A","CEC Survey",2017,15,"I",3091.5584807781133,"TON",8,{"v":1.6548264357155997,"d":"1.65"},{"$f":"VLOOKUP(A46771,cordwood_density!A:D,4,FALSE)","v":1.2726},{"v":1.3003508059999997,"d":"1.30"}]
["55141","55","WI","141","Wood","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",370.21078534044744,"A","CEC Survey",2017,15,"I",1511.9131285982003,"TON",8,{"v":4.083925127161918,"d":"4.08"},{"$f":"VLOOKUP(A46772,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.140031621683775,"d":"3.14"}]
["55141","55","WI","141","Wood","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",30.01709070327952,"A","CEC Survey",2017,15,"I",122.58755096742165,"TON",8,{"v":4.083925127161918,"d":"4.08"},{"$f":"VLOOKUP(A46773,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.140031621683775,"d":"3.14"}]
["55141","55","WI","141","Wood","","2104008610","Hydronic heater: outdoor","Hydronic heater",360.20508843935426,"A","CEC Survey",2017,15,"I",1471.0506116090596,"TON",8,{"v":4.083925127161917,"d":"4.08"},{"$f":"VLOOKUP(A46774,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.1400316216837747,"d":"3.14"}]
["55141","55","WI","141","Wood","","2104008620","Hydronic heater: indoor","Hydronic heater",230.131028725143,"A","CEC Survey",2017,15,"I",939.8378907502326,"TON",8,{"v":4.083925127161918,"d":"4.08"},{"$f":"VLOOKUP(A46775,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.140031621683775,"d":"3.14"}]
["55141","55","WI","141","Wood","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",10.005696901093174,"A","CEC Survey",2017,15,"I",40.86251698914055,"TON",8,{"v":4.083925127161918,"d":"4.08"},{"$f":"VLOOKUP(A46776,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":3.140031621683775,"d":"3.14"}]
["55141","55","WI","141","Wood","","2104008100","Fireplace: general","Fireplace: general",3797.369670657,"A","CEC Survey",2017,15,"I",1860.0149141873992,"TON",8,{"v":0.4898166561343999,"d":"0.49"},{"$f":"VLOOKUP(A46777,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.37660822399999994,"d":"0.38"}]
["55141","55","WI","141","Wood","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",183.98358834264,"A","CEC Survey",2017,15,"I",149.27993353533134,"TON",8,{"v":0.8113763563373998,"d":"0.81"},{"$f":"VLOOKUP(A46778,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.6238477289999999,"d":"0.62"}]
["55141","55","WI","141","Wood","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",812.59418184666,"A","CEC Survey",2017,15,"I",659.3197064477135,"TON",8,{"v":0.8113763563373999,"d":"0.81"},{"$f":"VLOOKUP(A46779,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.623847729,"d":"0.62"}]
["55141","55","WI","141","Wood","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",536.6187993327,"A","CEC Survey",2017,15,"I",435.3998061447164,"TON",8,{"v":0.8113763563373999,"d":"0.81"},{"$f":"VLOOKUP(A46780,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.623847729,"d":"0.62"}]
["55141","55","WI","141","Wood","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4534.704186845999,"A","CEC Survey",2017,15,"I",1845.9750080893582,"TON",8,{"v":0.407077271643,"d":"0.41"},{"$f":"VLOOKUP(A46781,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.312991905,"d":"0.31"}]
["55141","55","WI","141","Wood","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",1062.1857283470001,"A","CEC Survey",2017,15,"I",1064.4463113149402,"TON",8,{"v":1.002128237,"d":"1.00"},{"$f":"VLOOKUP(A46782,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.770512253575273,"d":"0.77"}]
["55141","55","WI","141","Wood","","2104009000","Wax Log; Total: All Combustor Types",null,31.38233617897972,"A","CEC Survey",2017,15,"I",17.291667234617826,"TON",8,{"v":0.551,"d":"0.55"},{"$f":"VLOOKUP(A46783,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":0.42365062278948185,"d":"0.42"}]
["55141","55","WI","141","Wood","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",465.28199134019997,"A","CEC Survey",2017,15,"I",945.0977448337949,"TON",8,{"v":2.0312364596608004,"d":"2.03"},{"$f":"VLOOKUP(A46784,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.5617687680000003,"d":"1.56"}]
["55141","55","WI","141","Wood","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",2054.99546175255,"A","CEC Survey",2017,15,"I",4174.181706349261,"TON",8,{"v":2.0312364596608,"d":"2.03"},{"$f":"VLOOKUP(A46785,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.5617687679999999,"d":"1.56"}]
["55141","55","WI","141","Wood","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",1357.0724747422498,"A","CEC Survey",2017,15,"I",2756.5350890985683,"TON",8,{"v":2.0312364596608004,"d":"2.03"},{"$f":"VLOOKUP(A46786,cordwood_density!A:D,4,FALSE)","v":1.3006},{"v":1.5617687680000003,"d":"1.56"}]
["56001","56","WY","001","Albany","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",93.79133272597227,"A","CEC Survey",2017,15,"I",162.73186805261523,"TON",8,{"$f":"P46787/J46787","v":{"v":1.7350416432194726,"d":"1.74"}},{"$f":"VLOOKUP(A46787,cordwood_density!A:D,4,FALSE)","v":1.017},{"$f":"S46787/T46787","v":{"v":1.7060389805501208,"d":"1.71"}}]
["56001","56","WY","001","Albany","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",7.604702653457211,"A","CEC Survey",2017,15,"I",13.194475788049884,"TON",8,{"v":1.7350416432194729,"d":"1.74"},{"$f":"VLOOKUP(A46788,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.706038980550121,"d":"1.71"}]
["56001","56","WY","001","Albany","","2104008610","Hydronic heater: outdoor","Hydronic heater",91.25643184148652,"A","CEC Survey",2017,15,"I",158.3337094565986,"TON",8,{"v":1.7350416432194729,"d":"1.74"},{"$f":"VLOOKUP(A46789,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.706038980550121,"d":"1.71"}]
["56001","56","WY","001","Albany","","2104008620","Hydronic heater: indoor","Hydronic heater",58.30272034317195,"A","CEC Survey",2017,15,"I",101.15764770838244,"TON",8,{"v":1.7350416432194729,"d":"1.74"},{"$f":"VLOOKUP(A46790,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.706038980550121,"d":"1.71"}]
["56001","56","WY","001","Albany","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.534900884485737,"A","CEC Survey",2017,15,"I",4.398158596016628,"TON",8,{"v":1.7350416432194726,"d":"1.74"},{"$f":"VLOOKUP(A46791,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7060389805501208,"d":"1.71"}]
["56001","56","WY","001","Albany","","2104008100","Fireplace: general","Fireplace: general",999.845809088,"A","CEC Survey",2017,15,"I",212.52005136205332,"TON",8,{"v":0.21255282507599996,"d":"0.21"},{"$f":"VLOOKUP(A46792,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.20899982799999997,"d":"0.21"}]
["56001","56","WY","001","Albany","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",149.36071841201002,"A","CEC Survey",2017,15,"I",36.62939443735585,"TON",8,{"v":0.24524115059699994,"d":"0.25"},{"$f":"VLOOKUP(A46793,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.24114174099999997,"d":"0.24"}]
["56001","56","WY","001","Albany","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",197.54159531911,"A","CEC Survey",2017,15,"I",48.44532812682548,"TON",8,{"v":0.24524115059699997,"d":"0.25"},{"$f":"VLOOKUP(A46794,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.241141741,"d":"0.24"}]
["56001","56","WY","001","Albany","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",134.90645533988,"A","CEC Survey",2017,15,"I",33.08461433051497,"TON",8,{"v":0.245241150597,"d":"0.25"},{"$f":"VLOOKUP(A46795,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.24114174100000002,"d":"0.24"}]
["56001","56","WY","001","Albany","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1510.220797624,"A","CEC Survey",2017,15,"I",257.6898873612564,"TON",8,{"v":0.17063060432399998,"d":"0.17"},{"$f":"VLOOKUP(A46796,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.167778372,"d":"0.17"}]
["56001","56","WY","001","Albany","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",323.383625026,"A","CEC Survey",2017,15,"I",119.04767308556892,"TON",8,{"v":0.36813142,"d":"0.37"},{"$f":"VLOOKUP(A46797,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.3619777974434612,"d":"0.36"}]
["56001","56","WY","001","Albany","","2104009000","Wax Log; Total: All Combustor Types",null,303.15224776007966,"A","CEC Survey",2017,15,"I",236.6086317241547,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46798,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["56001","56","WY","001","Albany","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",384.55046306971,"A","CEC Survey",2017,15,"I",299.36276039120105,"TON",8,{"v":0.7784745804269999,"d":"0.78"},{"$f":"VLOOKUP(A46799,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.765461731,"d":"0.77"}]
["56001","56","WY","001","Albany","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",508.59899954380995,"A","CEC Survey",2017,15,"I",395.9313927754594,"TON",8,{"v":0.778474580427,"d":"0.78"},{"$f":"VLOOKUP(A46800,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7654617310000001,"d":"0.77"}]
["56001","56","WY","001","Albany","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",347.33590212748004,"A","CEC Survey",2017,15,"I",270.3921706759235,"TON",8,{"v":0.7784745804269999,"d":"0.78"},{"$f":"VLOOKUP(A46801,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.765461731,"d":"0.77"}]
["56003","56","WY","003","Big Horn","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",86.29433417014516,"A","CEC Survey",2017,15,"I",161.33163532521505,"TON",8,{"v":1.8695507286390325,"d":"1.87"},{"$f":"VLOOKUP(A46802,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":1.7444720804693779,"d":"1.74"}]
["56003","56","WY","003","Big Horn","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.996837905687446,"A","CEC Survey",2017,15,"I",13.080943404747165,"TON",8,{"v":1.8695507286390323,"d":"1.87"},{"$f":"VLOOKUP(A46803,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":1.7444720804693776,"d":"1.74"}]
["56003","56","WY","003","Big Horn","","2104008610","Hydronic heater: outdoor","Hydronic heater",83.96205486824935,"A","CEC Survey",2017,15,"I",156.97132085696597,"TON",8,{"v":1.869550728639032,"d":"1.87"},{"$f":"VLOOKUP(A46804,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":1.7444720804693774,"d":"1.74"}]
["56003","56","WY","003","Big Horn","","2104008620","Hydronic heater: indoor","Hydronic heater",53.64242394360376,"A","CEC Survey",2017,15,"I",100.28723276972828,"TON",8,{"v":1.8695507286390323,"d":"1.87"},{"$f":"VLOOKUP(A46805,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":1.7444720804693776,"d":"1.74"}]
["56003","56","WY","003","Big Horn","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.3322793018958157,"A","CEC Survey",2017,15,"I",4.360314468249055,"TON",8,{"v":1.869550728639032,"d":"1.87"},{"$f":"VLOOKUP(A46806,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":1.7444720804693774,"d":"1.74"}]
["56003","56","WY","003","Big Horn","","2104008100","Fireplace: general","Fireplace: general",343.59309185100005,"A","CEC Survey",2017,15,"I",97.59289030992645,"TON",8,{"v":0.28403624119500004,"d":"0.28"},{"$f":"VLOOKUP(A46807,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.26503335,"d":"0.27"}]
["56003","56","WY","003","Big Horn","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",60.64343900986,"A","CEC Survey",2017,15,"I",15.425520765562835,"TON",8,{"v":0.2543642151141,"d":"0.25"},{"$f":"VLOOKUP(A46808,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.237346473,"d":"0.24"}]
["56003","56","WY","003","Big Horn","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",80.20583869046,"A","CEC Survey",2017,15,"I",20.401495206066972,"TON",8,{"v":0.2543642151141,"d":"0.25"},{"$f":"VLOOKUP(A46809,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.237346473,"d":"0.24"}]
["56003","56","WY","003","Big Horn","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",54.774719105680006,"A","CEC Survey",2017,15,"I",13.932728433411594,"TON",8,{"v":0.2543642151141,"d":"0.25"},{"$f":"VLOOKUP(A46810,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.237346473,"d":"0.24"}]
["56003","56","WY","003","Big Horn","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,689.790227232,"A","CEC Survey",2017,15,"I",126.79270566939906,"TON",8,{"v":0.1838134271316,"d":"0.18"},{"$f":"VLOOKUP(A46811,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.171515748,"d":"0.17"}]
["56003","56","WY","003","Big Horn","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",213.660913525,"A","CEC Survey",2017,15,"I",113.39886607586014,"TON",8,{"v":0.530742213,"d":"0.53"},{"$f":"VLOOKUP(A46812,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.4952339395353177,"d":"0.50"}]
["56003","56","WY","003","Big Horn","","2104009000","Wax Log; Total: All Combustor Types",null,84.85384609987614,"A","CEC Survey",2017,15,"I",66.22795169941516,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46813,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.7282769431743957,"d":"0.73"}]
["56003","56","WY","003","Big Horn","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",232.73765149195998,"A","CEC Survey",2017,15,"I",245.2418391580536,"TON",8,{"v":1.0537265353755003,"d":"1.05"},{"$f":"VLOOKUP(A46814,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.9832290150000003,"d":"0.98"}]
["56003","56","WY","003","Big Horn","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",307.81431326355994,"A","CEC Survey",2017,15,"I",324.3521098541999,"TON",8,{"v":1.0537265353755003,"d":"1.05"},{"$f":"VLOOKUP(A46815,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.9832290150000003,"d":"0.98"}]
["56003","56","WY","003","Big Horn","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",210.21465296048,"A","CEC Survey",2017,15,"I",221.50875794920972,"TON",8,{"v":1.0537265353755,"d":"1.05"},{"$f":"VLOOKUP(A46816,cordwood_density!A:D,4,FALSE)","v":1.0717},{"v":0.983229015,"d":"0.98"}]
["56005","56","WY","005","Campbell","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",137.17128143764864,"A","CEC Survey",2017,15,"I",249.10993233618615,"TON",8,{"v":1.8160501945111547,"d":"1.82"},{"$f":"VLOOKUP(A46817,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7672734473639107,"d":"1.77"}]
["56005","56","WY","005","Campbell","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.121995792241782,"A","CEC Survey",2017,15,"I",20.19810262185293,"TON",8,{"v":1.8160501945111545,"d":"1.82"},{"$f":"VLOOKUP(A46818,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7672734473639105,"d":"1.77"}]
["56005","56","WY","005","Campbell","","2104008610","Hydronic heater: outdoor","Hydronic heater",133.46394950690137,"A","CEC Survey",2017,15,"I",242.37723146223516,"TON",8,{"v":1.8160501945111547,"d":"1.82"},{"$f":"VLOOKUP(A46819,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7672734473639107,"d":"1.77"}]
["56005","56","WY","005","Campbell","","2104008620","Hydronic heater: indoor","Hydronic heater",85.268634407187,"A","CEC Survey",2017,15,"I",154.85212010087247,"TON",8,{"v":1.8160501945111547,"d":"1.82"},{"$f":"VLOOKUP(A46820,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7672734473639107,"d":"1.77"}]
["56005","56","WY","005","Campbell","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.7073319307472605,"A","CEC Survey",2017,15,"I",6.732700873950977,"TON",8,{"v":1.8160501945111547,"d":"1.82"},{"$f":"VLOOKUP(A46821,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7672734473639107,"d":"1.77"}]
["56005","56","WY","005","Campbell","","2104008100","Fireplace: general","Fireplace: general",935.8659046519999,"A","CEC Survey",2017,15,"I",215.48460906603466,"TON",8,{"v":0.2302515862528,"d":"0.23"},{"$f":"VLOOKUP(A46822,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22406732799999998,"d":"0.22"}]
["56005","56","WY","005","Campbell","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",197.47472263176002,"A","CEC Survey",2017,15,"I",43.09441623621741,"TON",8,{"v":0.21822750609240002,"d":"0.22"},{"$f":"VLOOKUP(A46823,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.212366199,"d":"0.21"}]
["56005","56","WY","005","Campbell","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",261.17624606136,"A","CEC Survey",2017,15,"I",56.99584082854561,"TON",8,{"v":0.21822750609240002,"d":"0.22"},{"$f":"VLOOKUP(A46824,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.212366199,"d":"0.21"}]
["56005","56","WY","005","Campbell","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",178.36426560288,"A","CEC Survey",2017,15,"I",38.92398885851896,"TON",8,{"v":0.21822750609240008,"d":"0.22"},{"$f":"VLOOKUP(A46825,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.21236619900000006,"d":"0.21"}]
["56005","56","WY","005","Campbell","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1827.8120933960001,"A","CEC Survey",2017,15,"I",317.5235036693422,"TON",8,{"v":0.17371780437200002,"d":"0.17"},{"$f":"VLOOKUP(A46826,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.16905197,"d":"0.17"}]
["56005","56","WY","005","Campbell","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",414.638190456,"A","CEC Survey",2017,15,"I",167.24772327562954,"TON",8,{"v":0.403358222,"d":"0.40"},{"$f":"VLOOKUP(A46827,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3925245445698715,"d":"0.39"}]
["56005","56","WY","005","Campbell","","2104009000","Wax Log; Total: All Combustor Types",null,333.05276616929734,"A","CEC Survey",2017,15,"I",259.945818899646,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46828,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["56005","56","WY","005","Campbell","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",546.59653318456,"A","CEC Survey",2017,15,"I",460.4586502795594,"TON",8,{"v":0.8424104843783999,"d":"0.84"},{"$f":"VLOOKUP(A46829,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8197844339999999,"d":"0.82"}]
["56005","56","WY","005","Campbell","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",722.91799550216,"A","CEC Survey",2017,15,"I",608.9936987568366,"TON",8,{"v":0.8424104843783999,"d":"0.84"},{"$f":"VLOOKUP(A46830,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8197844339999999,"d":"0.82"}]
["56005","56","WY","005","Campbell","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",493.70009448928005,"A","CEC Survey",2017,15,"I",415.8981357363763,"TON",8,{"v":0.8424104843784,"d":"0.84"},{"$f":"VLOOKUP(A46831,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.819784434,"d":"0.82"}]
["56007","56","WY","007","Carbon","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",74.53814715890027,"A","CEC Survey",2017,15,"I",134.94298887330396,"TON",8,{"v":1.810388291321929,"d":"1.81"},{"$f":"VLOOKUP(A46832,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7617636155332121,"d":"1.76"}]
["56007","56","WY","007","Carbon","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.043633553424346,"A","CEC Survey",2017,15,"I",10.94132342215978,"TON",8,{"v":1.810388291321929,"d":"1.81"},{"$f":"VLOOKUP(A46833,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7617636155332121,"d":"1.76"}]
["56007","56","WY","007","Carbon","","2104008610","Hydronic heater: outdoor","Hydronic heater",72.52360264109215,"A","CEC Survey",2017,15,"I",131.29588106591737,"TON",8,{"v":1.8103882913219291,"d":"1.81"},{"$f":"VLOOKUP(A46834,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7617636155332124,"d":"1.76"}]
["56007","56","WY","007","Carbon","","2104008620","Hydronic heater: indoor","Hydronic heater",46.33452390958666,"A","CEC Survey",2017,15,"I",83.88347956989166,"TON",8,{"v":1.8103882913219291,"d":"1.81"},{"$f":"VLOOKUP(A46835,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7617636155332124,"d":"1.76"}]
["56007","56","WY","007","Carbon","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.0145445178081154,"A","CEC Survey",2017,15,"I",3.6471078073865937,"TON",8,{"v":1.8103882913219291,"d":"1.81"},{"$f":"VLOOKUP(A46836,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7617636155332124,"d":"1.76"}]
["56007","56","WY","007","Carbon","","2104008100","Fireplace: general","Fireplace: general",446.466422835,"A","CEC Survey",2017,15,"I",105.38938142651821,"TON",8,{"v":0.23605220020200002,"d":"0.24"},{"$f":"VLOOKUP(A46837,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.229712145,"d":"0.23"}]
["56007","56","WY","007","Carbon","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",86.10136995855,"A","CEC Survey",2017,15,"I",20.85472551167955,"TON",8,{"v":0.2422113088528,"d":"0.24"},{"$f":"VLOOKUP(A46838,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.235705828,"d":"0.24"}]
["56007","56","WY","007","Carbon","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",113.87600542904998,"A","CEC Survey",2017,15,"I",27.58205632189876,"TON",8,{"v":0.24221130885280007,"d":"0.24"},{"$f":"VLOOKUP(A46839,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.23570582800000006,"d":"0.24"}]
["56007","56","WY","007","Carbon","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",77.76897931740001,"A","CEC Survey",2017,15,"I",18.83652626861379,"TON",8,{"v":0.24221130885280004,"d":"0.24"},{"$f":"VLOOKUP(A46840,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.23570582800000003,"d":"0.24"}]
["56007","56","WY","007","Carbon","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,833.881914525,"A","CEC Survey",2017,15,"I",147.36733638937721,"TON",8,{"v":0.1767244664052,"d":"0.18"},{"$f":"VLOOKUP(A46841,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.171977877,"d":"0.17"}]
["56007","56","WY","007","Carbon","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",213.69979046999998,"A","CEC Survey",2017,15,"I",98.95145096772684,"TON",8,{"v":0.463039532,"d":"0.46"},{"$f":"VLOOKUP(A46842,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.4506028921759439,"d":"0.45"}]
["56007","56","WY","007","Carbon","","2104009000","Wax Log; Total: All Combustor Types",null,117.5001372572487,"A","CEC Survey",2017,15,"I",91.70819912851395,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46843,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["56007","56","WY","007","Carbon","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",253.85196876444996,"A","CEC Survey",2017,15,"I",228.48820528142008,"TON",8,{"v":0.9000844326460001,"d":"0.90"},{"$f":"VLOOKUP(A46844,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8759093350000001,"d":"0.88"}]
["56007","56","WY","007","Carbon","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",335.73970062394994,"A","CEC Survey",2017,15,"I",302.19407795284593,"TON",8,{"v":0.9000844326460001,"d":"0.90"},{"$f":"VLOOKUP(A46845,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8759093350000001,"d":"0.88"}]
["56007","56","WY","007","Carbon","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",229.2856492066,"A","CEC Survey",2017,15,"I",206.37644347999236,"TON",8,{"v":0.9000844326460001,"d":"0.90"},{"$f":"VLOOKUP(A46846,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8759093350000001,"d":"0.88"}]
["56009","56","WY","009","Converse","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",50.04536909560831,"A","CEC Survey",2017,15,"I",86.90977280106169,"TON",8,{"v":1.7366196787364365,"d":"1.74"},{"$f":"VLOOKUP(A46847,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.707590637892268,"d":"1.71"}]
["56009","56","WY","009","Converse","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",4.057732629373646,"A","CEC Survey",2017,15,"I",7.046738335221217,"TON",8,{"v":1.7366196787364365,"d":"1.74"},{"$f":"VLOOKUP(A46848,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.707590637892268,"d":"1.71"}]
["56009","56","WY","009","Converse","","2104008610","Hydronic heater: outdoor","Hydronic heater",48.69279155248376,"A","CEC Survey",2017,15,"I",84.56086002265461,"TON",8,{"v":1.7366196787364363,"d":"1.74"},{"$f":"VLOOKUP(A46849,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7075906378922678,"d":"1.71"}]
["56009","56","WY","009","Converse","","2104008620","Hydronic heater: indoor","Hydronic heater",31.109283491864627,"A","CEC Survey",2017,15,"I",54.02499390336267,"TON",8,{"v":1.7366196787364363,"d":"1.74"},{"$f":"VLOOKUP(A46850,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7075906378922678,"d":"1.71"}]
["56009","56","WY","009","Converse","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.352577543124549,"A","CEC Survey",2017,15,"I",2.3489127784070725,"TON",8,{"$f":"P46851/J46851","v":{"v":1.736619678736436,"d":"1.74"}},{"$f":"VLOOKUP(A46851,cordwood_density!A:D,4,FALSE)","v":1.017},{"$f":"S46851/T46851","v":{"v":1.7075906378922676,"d":"1.71"}}]
["56009","56","WY","009","Converse","","2104008100","Fireplace: general","Fireplace: general",342.54504838915716,"A","CEC Survey",2017,15,"I",86.4527861176916,"TON",8,{"v":0.25238369821499995,"d":"0.25"},{"$f":"VLOOKUP(A46852,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.24816489499999997,"d":"0.25"}]
["56009","56","WY","009","Converse","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",70.01955106356313,"A","CEC Survey",2017,15,"I",15.849187671924525,"TON",8,{"v":0.22635374593499996,"d":"0.23"},{"$f":"VLOOKUP(A46853,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.222570055,"d":"0.22"}]
["56009","56","WY","009","Converse","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",92.60650301955123,"A","CEC Survey",2017,15,"I",20.961828856416307,"TON",8,{"v":0.226353745935,"d":"0.23"},{"$f":"VLOOKUP(A46854,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.22257005500000002,"d":"0.22"}]
["56009","56","WY","009","Converse","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",63.24346547676671,"A","CEC Survey",2017,15,"I",14.315395316576993,"TON",8,{"v":0.22635374593499996,"d":"0.23"},{"$f":"VLOOKUP(A46855,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.222570055,"d":"0.22"}]
["56009","56","WY","009","Converse","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,691.7992720671226,"A","CEC Survey",2017,15,"I",119.98571056899658,"TON",8,{"v":0.17344006479,"d":"0.17"},{"$f":"VLOOKUP(A46856,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17054087,"d":"0.17"}]
["56009","56","WY","009","Converse","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",177.73088016843144,"A","CEC Survey",2017,15,"I",63.92593283859553,"TON",8,{"v":0.359678255,"d":"0.36"},{"$f":"VLOOKUP(A46857,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.3536659341199607,"d":"0.35"}]
["56009","56","WY","009","Converse","","2104009000","Wax Log; Total: All Combustor Types",null,106.61172806459467,"A","CEC Survey",2017,15,"I",83.20985672873897,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46858,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["56009","56","WY","009","Converse","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",199.52190534366093,"A","CEC Survey",2017,15,"I",174.08669249888564,"TON",8,{"v":0.8725191963209998,"d":"0.87"},{"$f":"VLOOKUP(A46859,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.8579343129999999,"d":"0.86"}]
["56009","56","WY","009","Converse","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",263.883810293229,"A","CEC Survey",2017,15,"I",230.24369007917133,"TON",8,{"v":0.8725191963209998,"d":"0.87"},{"$f":"VLOOKUP(A46860,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.8579343129999999,"d":"0.86"}]
["56009","56","WY","009","Converse","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",180.21333385879055,"A","CEC Survey",2017,15,"I",157.23959322479996,"TON",8,{"v":0.8725191963209998,"d":"0.87"},{"$f":"VLOOKUP(A46861,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.8579343129999999,"d":"0.86"}]
["56011","56","WY","011","Crook","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",71.25880174106727,"A","CEC Survey",2017,15,"I",133.84188052138637,"TON",8,{"v":1.8782505073229676,"d":"1.88"},{"$f":"VLOOKUP(A46862,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.8369198115628045,"d":"1.84"}]
["56011","56","WY","011","Crook","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",5.777740681708158,"A","CEC Survey",2017,15,"I",10.852044366598896,"TON",8,{"v":1.8782505073229676,"d":"1.88"},{"$f":"VLOOKUP(A46863,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.8369198115628045,"d":"1.84"}]
["56011","56","WY","011","Crook","","2104008610","Hydronic heater: outdoor","Hydronic heater",69.33288818049789,"A","CEC Survey",2017,15,"I",130.22453239918676,"TON",8,{"v":1.8782505073229678,"d":"1.88"},{"$f":"VLOOKUP(A46864,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.8369198115628047,"d":"1.84"}]
["56011","56","WY","011","Crook","","2104008620","Hydronic heater: indoor","Hydronic heater",44.29601189309588,"A","CEC Survey",2017,15,"I",83.19900681059154,"TON",8,{"v":1.8782505073229676,"d":"1.88"},{"$f":"VLOOKUP(A46865,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.8369198115628045,"d":"1.84"}]
["56011","56","WY","011","Crook","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.925913560569386,"A","CEC Survey",2017,15,"I",3.617348122199632,"TON",8,{"v":1.8782505073229676,"d":"1.88"},{"$f":"VLOOKUP(A46866,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.8369198115628045,"d":"1.84"}]
["56011","56","WY","011","Crook","","2104008100","Fireplace: general","Fireplace: general",119.6395235,"A","CEC Survey",2017,15,"I",32.39455548368127,"TON",8,{"v":0.27076800822999997,"d":"0.27"},{"$f":"VLOOKUP(A46867,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":0.264809788,"d":"0.26"}]
["56011","56","WY","011","Crook","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",63.52185089950001,"A","CEC Survey",2017,15,"I",15.720288426455177,"TON",8,{"v":0.24747843779499998,"d":"0.25"},{"$f":"VLOOKUP(A46868,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":0.242032702,"d":"0.24"}]
["56011","56","WY","011","Crook","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",84.0127705445,"A","CEC Survey",2017,15,"I",20.791349209182652,"TON",8,{"v":0.247478437795,"d":"0.25"},{"$f":"VLOOKUP(A46869,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":0.24203270200000002,"d":"0.24"}]
["56011","56","WY","011","Crook","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",57.374575006000015,"A","CEC Survey",2017,15,"I",14.198970191636935,"TON",8,{"v":0.24747843779499998,"d":"0.25"},{"$f":"VLOOKUP(A46870,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":0.242032702,"d":"0.24"}]
["56011","56","WY","011","Crook","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,431.5971275,"A","CEC Survey",2017,15,"I",75.97765436428921,"TON",8,{"v":0.17603836893999997,"d":"0.18"},{"$f":"VLOOKUP(A46871,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":0.17216466399999997,"d":"0.17"}]
["56011","56","WY","011","Crook","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",131.29996551,"A","CEC Survey",2017,15,"I",102.22554858759553,"TON",8,{"v":0.778564931,"d":"0.78"},{"$f":"VLOOKUP(A46872,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":0.7614326953545233,"d":"0.76"}]
["56011","56","WY","011","Crook","","2104009000","Wax Log; Total: All Combustor Types",null,56.998454978939336,"A","CEC Survey",2017,15,"I",44.486974919714264,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46873,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":0.763319706601467,"d":"0.76"}]
["56011","56","WY","011","Crook","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",216.1394638886,"A","CEC Survey",2017,15,"I",221.3267304300045,"TON",8,{"v":1.0239996271299998,"d":"1.02"},{"$f":"VLOOKUP(A46874,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.0014666279999997,"d":"1.00"}]
["56011","56","WY","011","Crook","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",285.86187159459996,"A","CEC Survey",2017,15,"I",292.72244992355434,"TON",8,{"v":1.02399962713,"d":"1.02"},{"$f":"VLOOKUP(A46875,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.001466628,"d":"1.00"}]
["56011","56","WY","011","Crook","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",195.22274157680002,"A","CEC Survey",2017,15,"I",199.90801458193957,"TON",8,{"v":1.02399962713,"d":"1.02"},{"$f":"VLOOKUP(A46876,cordwood_density!A:D,4,FALSE)","v":1.0225},{"v":1.001466628,"d":"1.00"}]
["56013","56","WY","013","Fremont","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",213.37391944830082,"A","CEC Survey",2017,15,"I",390.14309696554847,"TON",8,{"v":1.8284479095397492,"d":"1.83"},{"$f":"VLOOKUP(A46877,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.797883883519911,"d":"1.80"}]
["56013","56","WY","013","Fremont","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",17.30058806337574,"A","CEC Survey",2017,15,"I",31.633224078287714,"TON",8,{"v":1.8284479095397492,"d":"1.83"},{"$f":"VLOOKUP(A46878,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.797883883519911,"d":"1.80"}]
["56013","56","WY","013","Fremont","","2104008610","Hydronic heater: outdoor","Hydronic heater",207.6070567605089,"A","CEC Survey",2017,15,"I",379.5986889394526,"TON",8,{"v":1.8284479095397494,"d":"1.83"},{"$f":"VLOOKUP(A46879,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7978838835199111,"d":"1.80"}]
["56013","56","WY","013","Fremont","","2104008620","Hydronic heater: indoor","Hydronic heater",132.63784181921403,"A","CEC Survey",2017,15,"I",242.52138460020583,"TON",8,{"v":1.8284479095397492,"d":"1.83"},{"$f":"VLOOKUP(A46880,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.797883883519911,"d":"1.80"}]
["56013","56","WY","013","Fremont","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.766862687791915,"A","CEC Survey",2017,15,"I",10.544408026095905,"TON",8,{"v":1.828447909539749,"d":"1.83"},{"$f":"VLOOKUP(A46881,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7978838835199107,"d":"1.80"}]
["56013","56","WY","013","Fremont","","2104008100","Fireplace: general","Fireplace: general",1004.814826857,"A","CEC Survey",2017,15,"I",237.714128659974,"TON",8,{"v":0.23657506070399997,"d":"0.24"},{"$f":"VLOOKUP(A46882,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.232620512,"d":"0.23"}]
["56013","56","WY","013","Fremont","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",216.16455280488,"A","CEC Survey",2017,15,"I",51.11904207023913,"TON",8,{"v":0.236482075377,"d":"0.24"},{"$f":"VLOOKUP(A46883,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.23252908100000003,"d":"0.23"}]
["56013","56","WY","013","Fremont","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",285.89505370968,"A","CEC Survey",2017,15,"I",67.609055641284,"TON",8,{"v":0.23648207537699997,"d":"0.24"},{"$f":"VLOOKUP(A46884,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.232529081,"d":"0.23"}]
["56013","56","WY","013","Fremont","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",195.24540253344003,"A","CEC Survey",2017,15,"I",46.17203799892567,"TON",8,{"v":0.23648207537699997,"d":"0.24"},{"$f":"VLOOKUP(A46885,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.232529081,"d":"0.23"}]
["56013","56","WY","013","Fremont","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,2040.318455345,"A","CEC Survey",2017,15,"I",355.5579948042032,"TON",8,{"v":0.17426593082699995,"d":"0.17"},{"$f":"VLOOKUP(A46886,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17135293099999996,"d":"0.17"}]
["56013","56","WY","013","Fremont","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",527.6840303629999,"A","CEC Survey",2017,15,"I",280.7474110486664,"TON",8,{"v":0.532036967,"d":"0.53"},{"$f":"VLOOKUP(A46887,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.5231435270403147,"d":"0.52"}]
["56013","56","WY","013","Fremont","","2104009000","Wax Log; Total: All Combustor Types",null,287.20782945700097,"A","CEC Survey",2017,15,"I",224.16410252734428,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46888,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["56013","56","WY","013","Fremont","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",676.2051761256,"A","CEC Survey",2017,15,"I",613.9508574822743,"TON",8,{"v":0.9079357555349998,"d":"0.91"},{"$f":"VLOOKUP(A46889,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.892758855,"d":"0.89"}]
["56013","56","WY","013","Fremont","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",894.3358781016,"A","CEC Survey",2017,15,"I",811.9995211862338,"TON",8,{"v":0.9079357555349999,"d":"0.91"},{"$f":"VLOOKUP(A46890,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.8927588550000001,"d":"0.89"}]
["56013","56","WY","013","Fremont","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",610.7659655328,"A","CEC Survey",2017,15,"I",554.5362583710865,"TON",8,{"v":0.907935755535,"d":"0.91"},{"$f":"VLOOKUP(A46891,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.8927588550000002,"d":"0.89"}]
["56015","56","WY","015","Goshen","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",48.83614130045355,"A","CEC Survey",2017,15,"I",83.86787411611326,"TON",8,{"v":1.7173321209006815,"d":"1.72"},{"$f":"VLOOKUP(A46892,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.671206812865591,"d":"1.67"}]
["56015","56","WY","015","Goshen","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.959687132469207,"A","CEC Survey",2017,15,"I",6.800097901306479,"TON",8,{"v":1.717332120900681,"d":"1.72"},{"$f":"VLOOKUP(A46893,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6712068128655906,"d":"1.67"}]
["56015","56","WY","015","Goshen","","2104008610","Hydronic heater: outdoor","Hydronic heater",47.51624558963048,"A","CEC Survey",2017,15,"I",81.60117481567775,"TON",8,{"v":1.7173321209006813,"d":"1.72"},{"$f":"VLOOKUP(A46894,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6712068128655908,"d":"1.67"}]
["56015","56","WY","015","Goshen","","2104008620","Hydronic heater: indoor","Hydronic heater",30.357601348930586,"A","CEC Survey",2017,15,"I",52.13408391001635,"TON",8,{"v":1.7173321209006813,"d":"1.72"},{"$f":"VLOOKUP(A46895,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6712068128655908,"d":"1.67"}]
["56015","56","WY","015","Goshen","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.319895710823069,"A","CEC Survey",2017,15,"I",2.2666993004354934,"TON",8,{"v":1.7173321209006813,"d":"1.72"},{"$f":"VLOOKUP(A46896,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6712068128655908,"d":"1.67"}]
["56015","56","WY","015","Goshen","","2104008100","Fireplace: general","Fireplace: general",379.05292497600004,"A","CEC Survey",2017,15,"I",93.07764378042279,"TON",8,{"v":0.2455531606472,"d":"0.25"},{"$f":"VLOOKUP(A46897,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.238957922,"d":"0.24"}]
["56015","56","WY","015","Goshen","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",73.46659756896,"A","CEC Survey",2017,15,"I",16.881111535642443,"TON",8,{"v":0.229779411246,"d":"0.23"},{"$f":"VLOOKUP(A46898,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22360783499999998,"d":"0.22"}]
["56015","56","WY","015","Goshen","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",97.16550001055998,"A","CEC Survey",2017,15,"I",22.326631385849684,"TON",8,{"v":0.22977941124600004,"d":"0.23"},{"$f":"VLOOKUP(A46899,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22360783500000003,"d":"0.22"}]
["56015","56","WY","015","Goshen","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",66.35692683648,"A","CEC Survey",2017,15,"I",15.247455580580272,"TON",8,{"v":0.22977941124600001,"d":"0.23"},{"$f":"VLOOKUP(A46900,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.223607835,"d":"0.22"}]
["56015","56","WY","015","Goshen","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,759.165333408,"A","CEC Survey",2017,15,"I",134.25855231592902,"TON",8,{"v":0.17685021484479999,"d":"0.18"},{"$f":"VLOOKUP(A46901,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.17210024799999998,"d":"0.17"}]
["56015","56","WY","015","Goshen","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",195.029644464,"A","CEC Survey",2017,15,"I",63.33695399338073,"TON",8,{"v":0.324755522,"d":"0.32"},{"$f":"VLOOKUP(A46902,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.31603301089918256,"d":"0.32"}]
["56015","56","WY","015","Goshen","","2104009000","Wax Log; Total: All Combustor Types",null,100.89294622185673,"A","CEC Survey",2017,15,"I",78.74637952566033,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46903,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["56015","56","WY","015","Goshen","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",199.03367344031997,"A","CEC Survey",2017,15,"I",167.35599678948955,"TON",8,{"v":0.8408426267612001,"d":"0.84"},{"$f":"VLOOKUP(A46904,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.818258687,"d":"0.82"}]
["56015","56","WY","015","Goshen","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",263.23808422751995,"A","CEC Survey",2017,15,"I",221.34180220545392,"TON",8,{"v":0.8408426267612001,"d":"0.84"},{"$f":"VLOOKUP(A46905,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.818258687,"d":"0.82"}]
["56015","56","WY","015","Goshen","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",179.77235020416,"A","CEC Survey",2017,15,"I",151.16025516470026,"TON",8,{"v":0.8408426267612,"d":"0.84"},{"$f":"VLOOKUP(A46906,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8182586869999999,"d":"0.82"}]
["56017","56","WY","017","Hot Springs","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",22.182774319959762,"A","CEC Survey",2017,15,"I",39.29020545066263,"TON",8,{"v":1.7712034069295757,"d":"1.77"},{"$f":"VLOOKUP(A46907,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7415962703338996,"d":"1.74"}]
["56017","56","WY","017","Hot Springs","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.7986033232399807,"A","CEC Survey",2017,15,"I",3.1856923338375105,"TON",8,{"v":1.7712034069295755,"d":"1.77"},{"$f":"VLOOKUP(A46908,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7415962703338994,"d":"1.74"}]
["56017","56","WY","017","Hot Springs","","2104008610","Hydronic heater: outdoor","Hydronic heater",21.58323987887977,"A","CEC Survey",2017,15,"I",38.22830800605013,"TON",8,{"v":1.7712034069295755,"d":"1.77"},{"$f":"VLOOKUP(A46909,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7415962703338994,"d":"1.74"}]
["56017","56","WY","017","Hot Springs","","2104008620","Hydronic heater: indoor","Hydronic heater",13.789292144839854,"A","CEC Survey",2017,15,"I",24.423641226087582,"TON",8,{"v":1.7712034069295755,"d":"1.77"},{"$f":"VLOOKUP(A46910,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7415962703338994,"d":"1.74"}]
["56017","56","WY","017","Hot Springs","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.5995344410799937,"A","CEC Survey",2017,15,"I",1.0618974446125036,"TON",8,{"v":1.7712034069295755,"d":"1.77"},{"$f":"VLOOKUP(A46911,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7415962703338994,"d":"1.74"}]
["56017","56","WY","017","Hot Springs","","2104008100","Fireplace: general","Fireplace: general",159.632071486,"A","CEC Survey",2017,15,"I",36.05472379420492,"TON",8,{"v":0.22586140403099997,"d":"0.23"},{"$f":"VLOOKUP(A46912,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.22208594299999998,"d":"0.22"}]
["56017","56","WY","017","Hot Springs","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",29.98249363834,"A","CEC Survey",2017,15,"I",6.9391669857632,"TON",8,{"v":0.23144062229999998,"d":"0.23"},{"$f":"VLOOKUP(A46913,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.2275719,"d":"0.23"}]
["56017","56","WY","017","Hot Springs","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",39.654265779739994,"A","CEC Survey",2017,15,"I",9.17760794891262,"TON",8,{"v":0.2314406223,"d":"0.23"},{"$f":"VLOOKUP(A46914,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.22757190000000002,"d":"0.23"}]
["56017","56","WY","017","Hot Springs","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",27.080961995920003,"A","CEC Survey",2017,15,"I",6.267634696818375,"TON",8,{"$f":"P46915/J46915","v":{"v":0.23144062229999998,"d":"0.23"}},{"$f":"VLOOKUP(A46915,cordwood_density!A:D,4,FALSE)","v":1.017},{"$f":"S46915/T46915","v":{"v":0.2275719,"d":"0.23"}}]
["56017","56","WY","017","Hot Springs","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,290.74781071,"A","CEC Survey",2017,15,"I",50.763200793609734,"TON",8,{"v":0.17459529848099997,"d":"0.17"},{"$f":"VLOOKUP(A46916,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.171676793,"d":"0.17"}]
["56017","56","WY","017","Hot Springs","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",69.84995989,"A","CEC Survey",2017,15,"I",28.797654290699256,"TON",8,{"v":0.412278752,"d":"0.41"},{"$f":"VLOOKUP(A46917,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.40538717010816133,"d":"0.41"}]
["56017","56","WY","017","Hot Springs","","2104009000","Wax Log; Total: All Combustor Types",null,42.53107305073015,"A","CEC Survey",2017,15,"I",33.19526434208579,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46918,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["56017","56","WY","017","Hot Springs","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",82.08267347336,"A","CEC Survey",2017,15,"I",69.19846098858663,"TON",8,{"v":0.8430337129679999,"d":"0.84"},{"$f":"VLOOKUP(A46919,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.828941704,"d":"0.83"}]
["56017","56","WY","017","Hot Springs","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",108.56095523896,"A","CEC Survey",2017,15,"I",91.52054517845329,"TON",8,{"v":0.8430337129679999,"d":"0.84"},{"$f":"VLOOKUP(A46920,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.828941704,"d":"0.83"}]
["56017","56","WY","017","Hot Springs","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",74.13918894368001,"A","CEC Survey",2017,15,"I",62.50183573162665,"TON",8,{"v":0.8430337129679999,"d":"0.84"},{"$f":"VLOOKUP(A46921,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.828941704,"d":"0.83"}]
["56019","56","WY","019","Johnson","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",45.08221699349358,"A","CEC Survey",2017,15,"I",83.44818668205717,"TON",8,{"v":1.8510222488415042,"d":"1.85"},{"$f":"VLOOKUP(A46922,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":1.7367444631652318,"d":"1.74"}]
["56019","56","WY","019","Johnson","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.6553148913643447,"A","CEC Survey",2017,15,"I",6.766069190437067,"TON",8,{"v":1.8510222488415038,"d":"1.85"},{"$f":"VLOOKUP(A46923,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":1.7367444631652313,"d":"1.74"}]
["56019","56","WY","019","Johnson","","2104008610","Hydronic heater: outdoor","Hydronic heater",43.86377869637214,"A","CEC Survey",2017,15,"I",81.19283028524481,"TON",8,{"v":1.851022248841504,"d":"1.85"},{"$f":"VLOOKUP(A46924,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":1.7367444631652316,"d":"1.74"}]
["56019","56","WY","019","Johnson","","2104008620","Hydronic heater: indoor","Hydronic heater",28.02408083379331,"A","CEC Survey",2017,15,"I",51.87319712668418,"TON",8,{"v":1.851022248841504,"d":"1.85"},{"$f":"VLOOKUP(A46925,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":1.7367444631652316,"d":"1.74"}]
["56019","56","WY","019","Johnson","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.2184382971214482,"A","CEC Survey",2017,15,"I",2.255356396812356,"TON",8,{"v":1.851022248841504,"d":"1.85"},{"$f":"VLOOKUP(A46926,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":1.7367444631652316,"d":"1.74"}]
["56019","56","WY","019","Johnson","","2104008100","Fireplace: general","Fireplace: general",271.95684407600004,"A","CEC Survey",2017,15,"I",67.38583837237411,"TON",8,{"v":0.24778136619920002,"d":"0.25"},{"$f":"VLOOKUP(A46927,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.232483924,"d":"0.23"}]
["56019","56","WY","019","Johnson","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",54.99980974596,"A","CEC Survey",2017,15,"I",14.207821661232616,"TON",8,{"v":0.2583249237926,"d":"0.26"},{"$f":"VLOOKUP(A46928,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.242376547,"d":"0.24"}]
["56019","56","WY","019","Johnson","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",72.74168385756,"A","CEC Survey",2017,15,"I",18.790989939049588,"TON",8,{"v":0.25832492379259997,"d":"0.26"},{"$f":"VLOOKUP(A46929,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.24237654699999994,"d":"0.24"}]
["56019","56","WY","019","Johnson","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",49.67724751248001,"A","CEC Survey",2017,15,"I",12.832871177887526,"TON",8,{"v":0.2583249237926,"d":"0.26"},{"$f":"VLOOKUP(A46930,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.242376547,"d":"0.24"}]
["56019","56","WY","019","Johnson","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,523.3577866080001,"A","CEC Survey",2017,15,"I",95.80470804752117,"TON",8,{"v":0.18305776755220002,"d":"0.18"},{"$f":"VLOOKUP(A46931,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.171756209,"d":"0.17"}]
["56019","56","WY","019","Johnson","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",135.70279804799998,"A","CEC Survey",2017,15,"I",60.96023452548509,"TON",8,{"v":0.4492187,"d":"0.45"},{"$f":"VLOOKUP(A46932,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.4214849878025896,"d":"0.42"}]
["56019","56","WY","019","Johnson","","2104009000","Wax Log; Total: All Combustor Types",null,71.54158236227003,"A","CEC Survey",2017,15,"I",55.837804400890526,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46933,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.7323085006567835,"d":"0.73"}]
["56019","56","WY","019","Johnson","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",158.43926591084,"A","CEC Survey",2017,15,"I",147.72715497940544,"TON",8,{"v":0.9323897969998001,"d":"0.93"},{"$f":"VLOOKUP(A46934,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.874826231,"d":"0.87"}]
["56019","56","WY","019","Johnson","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",209.54870652724,"A","CEC Survey",2017,15,"I",195.38107594050396,"TON",8,{"v":0.9323897969998,"d":"0.93"},{"$f":"VLOOKUP(A46935,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.8748262309999999,"d":"0.87"}]
["56019","56","WY","019","Johnson","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",143.10643372592003,"A","CEC Survey",2017,15,"I",133.4309786910759,"TON",8,{"v":0.9323897969998,"d":"0.93"},{"$f":"VLOOKUP(A46936,cordwood_density!A:D,4,FALSE)","v":1.0658},{"v":0.8748262309999999,"d":"0.87"}]
["56021","56","WY","021","Laramie","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",210.71534311150907,"A","CEC Survey",2017,15,"I",354.95705884112044,"TON",8,{"v":1.684533520908725,"d":"1.68"},{"$f":"VLOOKUP(A46937,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6392891406274086,"d":"1.64"}]
["56021","56","WY","021","Laramie","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",17.085027819852087,"A","CEC Survey",2017,15,"I",28.780302068198953,"TON",8,{"v":1.6845335209087249,"d":"1.68"},{"$f":"VLOOKUP(A46938,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6392891406274084,"d":"1.64"}]
["56021","56","WY","021","Laramie","","2104008610","Hydronic heater: outdoor","Hydronic heater",205.02033383822504,"A","CEC Survey",2017,15,"I",345.36362481838745,"TON",8,{"v":1.684533520908725,"d":"1.68"},{"$f":"VLOOKUP(A46939,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6392891406274086,"d":"1.64"}]
["56021","56","WY","021","Laramie","","2104008620","Hydronic heater: indoor","Hydronic heater",130.98521328553267,"A","CEC Survey",2017,15,"I",220.64898252285866,"TON",8,{"v":1.684533520908725,"d":"1.68"},{"$f":"VLOOKUP(A46940,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6392891406274086,"d":"1.64"}]
["56021","56","WY","021","Laramie","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",5.695009273284029,"A","CEC Survey",2017,15,"I",9.593434022732986,"TON",8,{"v":1.684533520908725,"d":"1.68"},{"$f":"VLOOKUP(A46941,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6392891406274086,"d":"1.64"}]
["56021","56","WY","021","Laramie","","2104008100","Fireplace: general","Fireplace: general",2891.9785341250004,"A","CEC Survey",2017,15,"I",681.1287101491622,"TON",8,{"v":0.23552343218040003,"d":"0.24"},{"$f":"VLOOKUP(A46942,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.229197579,"d":"0.23"}]
["56021","56","WY","021","Laramie","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",390.57864236771997,"A","CEC Survey",2017,15,"I",89.86250611604514,"TON",8,{"v":0.2300753199696,"d":"0.23"},{"$f":"VLOOKUP(A46943,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.223895796,"d":"0.22"}]
["56021","56","WY","021","Laramie","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",516.57175280892,"A","CEC Survey",2017,15,"I",118.85041131476937,"TON",8,{"v":0.23007531996959998,"d":"0.23"},{"$f":"VLOOKUP(A46944,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22389579599999998,"d":"0.22"}]
["56021","56","WY","021","Laramie","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",352.78070923536,"A","CEC Survey",2017,15,"I",81.16613455642788,"TON",8,{"v":0.2300753199696,"d":"0.23"},{"$f":"VLOOKUP(A46945,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.223895796,"d":"0.22"}]
["56021","56","WY","021","Laramie","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,4508.702066154,"A","CEC Survey",2017,15,"I",782.8463431110372,"TON",8,{"v":0.1736300894636,"d":"0.17"},{"$f":"VLOOKUP(A46946,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.168966611,"d":"0.17"}]
["56021","56","WY","021","Laramie","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",995.479797114,"A","CEC Survey",2017,15,"I",259.5623748832661,"TON",8,{"v":0.260740977,"d":"0.26"},{"$f":"VLOOKUP(A46947,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.2537378133514986,"d":"0.25"}]
["56021","56","WY","021","Laramie","","2104009000","Wax Log; Total: All Combustor Types",null,728.0463782642129,"A","CEC Survey",2017,15,"I",568.2361211754998,"TON",8,{"v":0.7804943999999998,"d":"0.78"},{"$f":"VLOOKUP(A46948,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498635,"d":"0.76"}]
["56021","56","WY","021","Laramie","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",959.6702294029901,"A","CEC Survey",2017,15,"I",730.8825626068108,"TON",8,{"v":0.7615976199048001,"d":"0.76"},{"$f":"VLOOKUP(A46949,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7411420980000001,"d":"0.74"}]
["56021","56","WY","021","Laramie","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1269.24127114589,"A","CEC Survey",2017,15,"I",966.6511311896529,"TON",8,{"v":0.7615976199048001,"d":"0.76"},{"$f":"VLOOKUP(A46950,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7411420980000001,"d":"0.74"}]
["56021","56","WY","021","Laramie","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",866.7989168801201,"A","CEC Survey",2017,15,"I",660.1519920319581,"TON",8,{"v":0.7615976199048,"d":"0.76"},{"$f":"VLOOKUP(A46951,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.741142098,"d":"0.74"}]
["56023","56","WY","023","Lincoln","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",171.61739624358844,"A","CEC Survey",2017,15,"I",321.9144937555117,"TON",8,{"v":1.875768429085104,"d":"1.88"},{"$f":"VLOOKUP(A46952,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":1.8406127260181573,"d":"1.84"}]
["56023","56","WY","023","Lincoln","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.914924019750416,"A","CEC Survey",2017,15,"I",26.101175169365813,"TON",8,{"v":1.8757684290851038,"d":"1.88"},{"$f":"VLOOKUP(A46953,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":1.840612726018157,"d":"1.84"}]
["56023","56","WY","023","Lincoln","","2104008610","Hydronic heater: outdoor","Hydronic heater",166.979088237005,"A","CEC Survey",2017,15,"I",313.21410203238975,"TON",8,{"v":1.8757684290851036,"d":"1.88"},{"$f":"VLOOKUP(A46954,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":1.8406127260181568,"d":"1.84"}]
["56023","56","WY","023","Lincoln","","2104008620","Hydronic heater: indoor","Hydronic heater",106.68108415141985,"A","CEC Survey",2017,15,"I",200.10900963180458,"TON",8,{"v":1.8757684290851038,"d":"1.88"},{"$f":"VLOOKUP(A46955,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":1.840612726018157,"d":"1.84"}]
["56023","56","WY","023","Lincoln","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.638308006583472,"A","CEC Survey",2017,15,"I",8.700391723121939,"TON",8,{"v":1.875768429085104,"d":"1.88"},{"$f":"VLOOKUP(A46956,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":1.8406127260181573,"d":"1.84"}]
["56023","56","WY","023","Lincoln","","2104008100","Fireplace: general","Fireplace: general",391.70112539545823,"A","CEC Survey",2017,15,"I",99.81557143929761,"TON",8,{"v":0.2548258479945,"d":"0.25"},{"$f":"VLOOKUP(A46957,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.250049895,"d":"0.25"}]
["56023","56","WY","023","Lincoln","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",136.7445278506707,"A","CEC Survey",2017,15,"I",36.22969899902312,"TON",8,{"v":0.264944415462,"d":"0.26"},{"$f":"VLOOKUP(A46958,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.25997882,"d":"0.26"}]
["56023","56","WY","023","Lincoln","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",180.85566586701609,"A","CEC Survey",2017,15,"I",47.91669867612735,"TON",8,{"v":0.2649444154619999,"d":"0.26"},{"$f":"VLOOKUP(A46959,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.25997881999999994,"d":"0.26"}]
["56023","56","WY","023","Lincoln","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",123.5111864457671,"A","CEC Survey",2017,15,"I",32.723599095891856,"TON",8,{"v":0.264944415462,"d":"0.26"},{"$f":"VLOOKUP(A46960,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.25997882,"d":"0.26"}]
["56023","56","WY","023","Lincoln","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1088.1935920170697,"A","CEC Survey",2017,15,"I",190.11250204667581,"TON",8,{"v":0.174704669685,"d":"0.17"},{"$f":"VLOOKUP(A46961,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.17143035000000004,"d":"0.17"}]
["56023","56","WY","023","Lincoln","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",317.8693544770049,"A","CEC Survey",2017,15,"I",248.03530062279353,"TON",8,{"v":0.780305799,"d":"0.78"},{"$f":"VLOOKUP(A46962,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.7656812864292023,"d":"0.77"}]
["56023","56","WY","023","Lincoln","","2104009000","Wax Log; Total: All Combustor Types",null,133.74753739974983,"A","CEC Survey",2017,15,"I",104.3892039542953,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46963,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.7658663526641154,"d":"0.77"}]
["56023","56","WY","023","Lincoln","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",471.40343561622274,"A","CEC Survey",2017,15,"I",465.89568394883315,"TON",8,{"v":0.9883162674446999,"d":"0.99"},{"$f":"VLOOKUP(A46964,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.969793217,"d":"0.97"}]
["56023","56","WY","023","Lincoln","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",623.4690600085526,"A","CEC Survey",2017,15,"I",616.1846142549083,"TON",8,{"v":0.9883162674446999,"d":"0.99"},{"$f":"VLOOKUP(A46965,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.969793217,"d":"0.97"}]
["56023","56","WY","023","Lincoln","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",425.7837482985238,"A","CEC Survey",2017,15,"I",420.8090048570106,"TON",8,{"v":0.9883162674446999,"d":"0.99"},{"$f":"VLOOKUP(A46966,cordwood_density!A:D,4,FALSE)","v":1.0191},{"v":0.969793217,"d":"0.97"}]
["56025","56","WY","025","Natrona","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",169.47853736372429,"A","CEC Survey",2017,15,"I",281.8225808315148,"TON",8,{"v":1.662880652708754,"d":"1.66"},{"$f":"VLOOKUP(A46967,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.6350842209525607,"d":"1.64"}]
["56025","56","WY","025","Natrona","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",13.74150302949116,"A","CEC Survey",2017,15,"I",22.85047952687958,"TON",8,{"v":1.662880652708754,"d":"1.66"},{"$f":"VLOOKUP(A46968,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.6350842209525607,"d":"1.64"}]
["56025","56","WY","025","Natrona","","2104008610","Hydronic heater: outdoor","Hydronic heater",164.8980363538939,"A","CEC Survey",2017,15,"I",274.205754322555,"TON",8,{"v":1.6628806527087543,"d":"1.66"},{"$f":"VLOOKUP(A46969,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.635084220952561,"d":"1.64"}]
["56025","56","WY","025","Natrona","","2104008620","Hydronic heater: indoor","Hydronic heater",105.35152322609889,"A","CEC Survey",2017,15,"I",175.1870097060768,"TON",8,{"v":1.662880652708754,"d":"1.66"},{"$f":"VLOOKUP(A46970,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.6350842209525607,"d":"1.64"}]
["56025","56","WY","025","Natrona","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",4.580501009830386,"A","CEC Survey",2017,15,"I",7.616826508959861,"TON",8,{"v":1.6628806527087543,"d":"1.66"},{"$f":"VLOOKUP(A46971,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.635084220952561,"d":"1.64"}]
["56025","56","WY","025","Natrona","","2104008100","Fireplace: general","Fireplace: general",2563.717121672,"A","CEC Survey",2017,15,"I",567.245684840378,"TON",8,{"v":0.221259077316,"d":"0.22"},{"$f":"VLOOKUP(A46972,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.21756054800000002,"d":"0.22"}]
["56025","56","WY","025","Natrona","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",352.6303409776,"A","CEC Survey",2017,15,"I",80.150104102252,"TON",8,{"v":0.227292137937,"d":"0.23"},{"$f":"VLOOKUP(A46973,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.22349276100000004,"d":"0.22"}]
["56025","56","WY","025","Natrona","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",466.3820638736,"A","CEC Survey",2017,15,"I",106.00497639330102,"TON",8,{"v":0.22729213793699998,"d":"0.23"},{"$f":"VLOOKUP(A46974,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.223492761,"d":"0.22"}]
["56025","56","WY","025","Natrona","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",318.50482410880005,"A","CEC Survey",2017,15,"I",72.39364241493729,"TON",8,{"v":0.22729213793699996,"d":"0.23"},{"$f":"VLOOKUP(A46975,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.22349276099999998,"d":"0.22"}]
["56025","56","WY","025","Natrona","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,3877.7758342399998,"A","CEC Survey",2017,15,"I",675.6741057361428,"TON",8,{"v":0.17424269339399998,"d":"0.17"},{"$f":"VLOOKUP(A46976,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.171330082,"d":"0.17"}]
["56025","56","WY","025","Natrona","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",857.91334524,"A","CEC Survey",2017,15,"I",213.82352193845873,"TON",8,{"v":0.249236736,"d":"0.25"},{"$f":"VLOOKUP(A46977,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.24507053687315636,"d":"0.25"}]
["56025","56","WY","025","Natrona","","2104009000","Wax Log; Total: All Combustor Types",null,624.597022932005,"A","CEC Survey",2017,15,"I",487.49447865510143,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46978,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["56025","56","WY","025","Natrona","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",815.1739416570399,"A","CEC Survey",2017,15,"I",608.2270470136423,"TON",8,{"$f":"P46979/J46979","v":{"v":0.746131611834,"d":"0.75"}},{"$f":"VLOOKUP(A46979,cordwood_density!A:D,4,FALSE)","v":1.017},{"$f":"S46979/T46979","v":{"v":0.7336594020000001,"d":"0.73"}}]
["56025","56","WY","025","Natrona","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",1078.1332776754398,"A","CEC Survey",2017,15,"I",804.4293202438494,"TON",8,{"v":0.746131611834,"d":"0.75"},{"$f":"VLOOKUP(A46980,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7336594020000001,"d":"0.73"}]
["56025","56","WY","025","Natrona","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",736.28614085152,"A","CEC Survey",2017,15,"I",549.3663650445801,"TON",8,{"v":0.7461316118339999,"d":"0.75"},{"$f":"VLOOKUP(A46981,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.733659402,"d":"0.73"}]
["56027","56","WY","027","Niobrara","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",17.213086391697423,"A","CEC Survey",2017,15,"I",30.57974278627519,"TON",8,{"v":1.776540365301661,"d":"1.78"},{"$f":"VLOOKUP(A46982,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.728824800799592,"d":"1.73"}]
["56027","56","WY","027","Niobrara","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",1.3956556533808722,"A","CEC Survey",2017,15,"I",2.4794386042925827,"TON",8,{"v":1.7765403653016607,"d":"1.78"},{"$f":"VLOOKUP(A46983,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7288248007995919,"d":"1.73"}]
["56027","56","WY","027","Niobrara","","2104008610","Hydronic heater: outdoor","Hydronic heater",16.747867840570464,"A","CEC Survey",2017,15,"I",29.753263251510994,"TON",8,{"v":1.7765403653016612,"d":"1.78"},{"$f":"VLOOKUP(A46984,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7288248007995923,"d":"1.73"}]
["56027","56","WY","027","Niobrara","","2104008620","Hydronic heater: indoor","Hydronic heater",10.70002667592002,"A","CEC Survey",2017,15,"I",19.00902929957647,"TON",8,{"v":1.776540365301661,"d":"1.78"},{"$f":"VLOOKUP(A46985,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.728824800799592,"d":"1.73"}]
["56027","56","WY","027","Niobrara","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.4652185511269574,"A","CEC Survey",2017,15,"I",0.8264795347641943,"TON",8,{"v":1.776540365301661,"d":"1.78"},{"$f":"VLOOKUP(A46986,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.728824800799592,"d":"1.73"}]
["56027","56","WY","027","Niobrara","","2104008100","Fireplace: general","Fireplace: general",56.52242736,"A","CEC Survey",2017,15,"I",15.818941871123018,"TON",8,{"v":0.279870179148,"d":"0.28"},{"$f":"VLOOKUP(A46987,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.27235323,"d":"0.27"}]
["56027","56","WY","027","Niobrara","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",15.2723967507,"A","CEC Survey",2017,15,"I",3.482187841106858,"TON",8,{"v":0.2280053286952,"d":"0.23"},{"$f":"VLOOKUP(A46988,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22188140199999998,"d":"0.22"}]
["56027","56","WY","027","Niobrara","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",20.198976347699997,"A","CEC Survey",2017,15,"I",4.605474241463909,"TON",8,{"v":0.22800532869520007,"d":"0.23"},{"$f":"VLOOKUP(A46989,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22188140200000006,"d":"0.22"}]
["56027","56","WY","027","Niobrara","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",13.794422871600002,"A","CEC Survey",2017,15,"I",3.1452019209997433,"TON",8,{"v":0.22800532869520002,"d":"0.23"},{"$f":"VLOOKUP(A46990,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.221881402,"d":"0.22"}]
["56027","56","WY","027","Niobrara","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,152.627024958,"A","CEC Survey",2017,15,"I",27.02824010314555,"TON",8,{"v":0.17708685673840002,"d":"0.18"},{"$f":"VLOOKUP(A46991,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.172330534,"d":"0.17"}]
["56027","56","WY","027","Niobrara","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",47.954645282,"A","CEC Survey",2017,15,"I",22.798019702402083,"TON",8,{"v":0.475407952,"d":"0.48"},{"$f":"VLOOKUP(A46992,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.4626391124951343,"d":"0.46"}]
["56027","56","WY","027","Niobrara","","2104009000","Wax Log; Total: All Combustor Types",null,18.595509232331704,"A","CEC Survey",2017,15,"I",14.513690820983193,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A46993,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["56027","56","WY","027","Niobrara","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",54.819195898619995,"A","CEC Survey",2017,15,"I",53.36735046097232,"TON",8,{"v":0.9735157472880002,"d":"0.97"},{"$f":"VLOOKUP(A46994,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9473683800000001,"d":"0.95"}]
["56027","56","WY","027","Niobrara","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",72.50280747881999,"A","CEC Survey",2017,15,"I",70.58262480322145,"TON",8,{"v":0.9735157472880002,"d":"0.97"},{"$f":"VLOOKUP(A46995,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.9473683800000001,"d":"0.95"}]
["56027","56","WY","027","Niobrara","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",49.514112424560004,"A","CEC Survey",2017,15,"I",48.20276815829758,"TON",8,{"v":0.973515747288,"d":"0.97"},{"$f":"VLOOKUP(A46996,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.94736838,"d":"0.95"}]
["56029","56","WY","029","Park","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",147.15811249378515,"A","CEC Survey",2017,15,"I",265.5656834633717,"TON",8,{"v":1.8046282258111133,"d":"1.80"},{"$f":"VLOOKUP(A46997,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":1.7643999079107484,"d":"1.76"}]
["56029","56","WY","029","Park","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",11.931738850847445,"A","CEC Survey",2017,15,"I",21.532352713246357,"TON",8,{"v":1.8046282258111133,"d":"1.80"},{"$f":"VLOOKUP(A46998,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":1.7643999079107484,"d":"1.76"}]
["56029","56","WY","029","Park","","2104008610","Hydronic heater: outdoor","Hydronic heater",143.18086621016934,"A","CEC Survey",2017,15,"I",258.3882325589563,"TON",8,{"v":1.8046282258111135,"d":"1.80"},{"$f":"VLOOKUP(A46999,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":1.7643999079107486,"d":"1.76"}]
["56029","56","WY","029","Park","","2104008620","Hydronic heater: indoor","Hydronic heater",91.47666452316375,"A","CEC Survey",2017,15,"I",165.0813708015554,"TON",8,{"v":1.8046282258111133,"d":"1.80"},{"$f":"VLOOKUP(A47000,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":1.7643999079107484,"d":"1.76"}]
["56029","56","WY","029","Park","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.977246283615815,"A","CEC Survey",2017,15,"I",7.177450904415452,"TON",8,{"v":1.8046282258111133,"d":"1.80"},{"$f":"VLOOKUP(A47001,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":1.7643999079107484,"d":"1.76"}]
["56029","56","WY","029","Park","","2104008100","Fireplace: general","Fireplace: general",1098.282460911,"A","CEC Survey",2017,15,"I",261.43463209751104,"TON",8,{"v":0.238039522074,"d":"0.24"},{"$f":"VLOOKUP(A47002,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.23273320500000003,"d":"0.23"}]
["56029","56","WY","029","Park","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",156.8528272386,"A","CEC Survey",2017,15,"I",43.063482878226125,"TON",8,{"v":0.27454706195839995,"d":"0.27"},{"$f":"VLOOKUP(A47003,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.26842692799999995,"d":"0.27"}]
["56029","56","WY","029","Park","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",207.4505134446,"A","CEC Survey",2017,15,"I",56.954928967976485,"TON",8,{"v":0.27454706195839995,"d":"0.27"},{"$f":"VLOOKUP(A47004,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.26842692799999995,"d":"0.27"}]
["56029","56","WY","029","Park","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",141.6735213768,"A","CEC Survey",2017,15,"I",38.89604905130102,"TON",8,{"v":0.2745470619584,"d":"0.27"},{"$f":"VLOOKUP(A47005,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.268426928,"d":"0.27"}]
["56029","56","WY","029","Park","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1654.078971363,"A","CEC Survey",2017,15,"I",288.4227147670659,"TON",8,{"v":0.1743705831224,"d":"0.17"},{"$f":"VLOOKUP(A47006,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.170483558,"d":"0.17"}]
["56029","56","WY","029","Park","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",410.508537249,"A","CEC Survey",2017,15,"I",199.30471995414285,"TON",8,{"v":0.485506882,"d":"0.49"},{"$f":"VLOOKUP(A47007,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.47468408486507624,"d":"0.47"}]
["56029","56","WY","029","Park","","2104009000","Wax Log; Total: All Combustor Types",null,223.65739261005066,"A","CEC Survey",2017,15,"I",174.56334245074592,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47008,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.763095815408682,"d":"0.76"}]
["56029","56","WY","029","Park","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",464.30193753599997,"A","CEC Survey",2017,15,"I",414.6881658738669,"TON",8,{"v":0.8931433025556,"d":"0.89"},{"$f":"VLOOKUP(A47009,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.8732335770000001,"d":"0.87"}]
["56029","56","WY","029","Park","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",614.0767560959999,"A","CEC Survey",2017,15,"I",548.458541962211,"TON",8,{"v":0.8931433025555999,"d":"0.89"},{"$f":"VLOOKUP(A47010,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.873233577,"d":"0.87"}]
["56029","56","WY","029","Park","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",419.36949196800003,"A","CEC Survey",2017,15,"I",374.5570530473637,"TON",8,{"v":0.8931433025555999,"d":"0.89"},{"$f":"VLOOKUP(A47011,cordwood_density!A:D,4,FALSE)","v":1.0228},{"v":0.873233577,"d":"0.87"}]
["56031","56","WY","031","Platte","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",40.4220394610528,"A","CEC Survey",2017,15,"I",70.3627449840826,"TON",8,{"v":1.740702496020224,"d":"1.74"},{"$f":"VLOOKUP(A47012,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6939494900936394,"d":"1.69"}]
["56031","56","WY","031","Platte","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.277462659004281,"A","CEC Survey",2017,15,"I",5.705087431141832,"TON",8,{"v":1.7407024960202242,"d":"1.74"},{"$f":"VLOOKUP(A47013,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6939494900936396,"d":"1.69"}]
["56031","56","WY","031","Platte","","2104008610","Hydronic heater: outdoor","Hydronic heater",39.32955190805137,"A","CEC Survey",2017,15,"I",68.46104917370198,"TON",8,{"v":1.7407024960202238,"d":"1.74"},{"$f":"VLOOKUP(A47014,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6939494900936392,"d":"1.69"}]
["56031","56","WY","031","Platte","","2104008620","Hydronic heater: indoor","Hydronic heater",25.127213719032824,"A","CEC Survey",2017,15,"I",43.73900363875405,"TON",8,{"v":1.740702496020224,"d":"1.74"},{"$f":"VLOOKUP(A47015,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6939494900936394,"d":"1.69"}]
["56031","56","WY","031","Platte","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.092487553001427,"A","CEC Survey",2017,15,"I",1.9016958103806108,"TON",8,{"v":1.740702496020224,"d":"1.74"},{"$f":"VLOOKUP(A47016,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.6939494900936394,"d":"1.69"}]
["56031","56","WY","031","Platte","","2104008100","Fireplace: general","Fireplace: general",241.9286395446868,"A","CEC Survey",2017,15,"I",61.52033301990024,"TON",8,{"v":0.254291237018,"d":"0.25"},{"$f":"VLOOKUP(A47017,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.24746130499999996,"d":"0.25"}]
["56031","56","WY","031","Platte","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",55.30589707218767,"A","CEC Survey",2017,15,"I",12.862346072414423,"TON",8,{"v":0.23256735272960002,"d":"0.23"},{"$f":"VLOOKUP(A47018,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22632089600000002,"d":"0.23"}]
["56031","56","WY","031","Platte","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",73.14650903095789,"A","CEC Survey",2017,15,"I",17.011489966741657,"TON",8,{"v":0.23256735272960002,"d":"0.23"},{"$f":"VLOOKUP(A47019,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22632089600000002,"d":"0.23"}]
["56031","56","WY","031","Platte","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",49.95371348455661,"A","CEC Survey",2017,15,"I",11.617602904116255,"TON",8,{"v":0.23256735272960005,"d":"0.23"},{"$f":"VLOOKUP(A47020,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22632089600000005,"d":"0.23"}]
["56031","56","WY","031","Platte","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,533.3444242826054,"A","CEC Survey",2017,15,"I",94.33676689575312,"TON",8,{"v":0.17687775966280003,"d":"0.18"},{"$f":"VLOOKUP(A47021,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.17212705300000003,"d":"0.17"}]
["56031","56","WY","031","Platte","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",143.6252714984025,"A","CEC Survey",2017,15,"I",53.519237448488056,"TON",8,{"v":0.372631062,"d":"0.37"},{"$f":"VLOOKUP(A47022,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3626226761385753,"d":"0.36"}]
["56031","56","WY","031","Platte","","2104009000","Wax Log; Total: All Combustor Types",null,70.82200055755202,"A","CEC Survey",2017,15,"I",55.27617483196622,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47023,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["56031","56","WY","031","Platte","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",157.53837234772254,"A","CEC Survey",2017,15,"I",139.546923033279,"TON",8,{"v":0.8857963996560001,"d":"0.89"},{"$f":"VLOOKUP(A47024,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.86200506,"d":"0.86"}]
["56031","56","WY","031","Platte","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",208.35720213731045,"A","CEC Survey",2017,15,"I",184.56205949562707,"TON",8,{"v":0.8857963996560002,"d":"0.89"},{"$f":"VLOOKUP(A47025,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8620050600000001,"d":"0.86"}]
["56031","56","WY","031","Platte","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",142.29272341084618,"A","CEC Survey",2017,15,"I",126.0423820945746,"TON",8,{"v":0.8857963996560002,"d":"0.89"},{"$f":"VLOOKUP(A47026,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8620050600000001,"d":"0.86"}]
["56033","56","WY","033","Sheridan","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",134.7271498693797,"A","CEC Survey",2017,15,"I",237.93726224721897,"TON",8,{"v":1.766067659546745,"d":"1.77"},{"$f":"VLOOKUP(A47027,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7365463712357376,"d":"1.74"}]
["56033","56","WY","033","Sheridan","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",10.923822962382136,"A","CEC Survey",2017,15,"I",19.292210452477214,"TON",8,{"v":1.7660676595467453,"d":"1.77"},{"$f":"VLOOKUP(A47028,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7365463712357379,"d":"1.74"}]
["56033","56","WY","033","Sheridan","","2104008610","Hydronic heater: outdoor","Hydronic heater",131.08587554858565,"A","CEC Survey",2017,15,"I",231.50652542972657,"TON",8,{"v":1.7660676595467453,"d":"1.77"},{"$f":"VLOOKUP(A47029,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7365463712357379,"d":"1.74"}]
["56033","56","WY","033","Sheridan","","2104008620","Hydronic heater: indoor","Hydronic heater",83.74930937826305,"A","CEC Survey",2017,15,"I",147.9069468023253,"TON",8,{"v":1.7660676595467453,"d":"1.77"},{"$f":"VLOOKUP(A47030,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7365463712357379,"d":"1.74"}]
["56033","56","WY","033","Sheridan","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",3.6412743207940457,"A","CEC Survey",2017,15,"I",6.430736817492405,"TON",8,{"v":1.7660676595467453,"d":"1.77"},{"$f":"VLOOKUP(A47031,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7365463712357379,"d":"1.74"}]
["56033","56","WY","033","Sheridan","","2104008100","Fireplace: general","Fireplace: general",1061.42461763,"A","CEC Survey",2017,15,"I",241.29631903606676,"TON",8,{"v":0.22733250673499997,"d":"0.23"},{"$f":"VLOOKUP(A47032,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.223532455,"d":"0.22"}]
["56033","56","WY","033","Sheridan","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",183.7114966999,"A","CEC Survey",2017,15,"I",49.24560172351009,"TON",8,{"v":0.268059444336,"d":"0.27"},{"$f":"VLOOKUP(A47033,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.263578608,"d":"0.26"}]
["56033","56","WY","033","Sheridan","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",242.97326982890002,"A","CEC Survey",2017,15,"I",65.13127969883593,"TON",8,{"v":0.268059444336,"d":"0.27"},{"$f":"VLOOKUP(A47034,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.263578608,"d":"0.26"}]
["56033","56","WY","033","Sheridan","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",165.93296476120003,"A","CEC Survey",2017,15,"I",44.47989833091235,"TON",8,{"v":0.268059444336,"d":"0.27"},{"$f":"VLOOKUP(A47035,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.263578608,"d":"0.26"}]
["56033","56","WY","033","Sheridan","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1763.0543183500001,"A","CEC Survey",2017,15,"I",307.29547151025747,"TON",8,{"v":0.17429722289999997,"d":"0.17"},{"$f":"VLOOKUP(A47036,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17138369999999997,"d":"0.17"}]
["56033","56","WY","033","Sheridan","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",426.91174799000004,"A","CEC Survey",2017,15,"I",187.2118491158295,"TON",8,{"v":0.438525878,"d":"0.44"},{"$f":"VLOOKUP(A47037,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.43119555358898726,"d":"0.43"}]
["56033","56","WY","033","Sheridan","","2104009000","Wax Log; Total: All Combustor Types",null,248.63445643636993,"A","CEC Survey",2017,15,"I",194.05780089563066,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47038,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["56033","56","WY","033","Sheridan","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",491.94763504379995,"A","CEC Survey",2017,15,"I",416.38292546295077,"TON",8,{"v":0.8463968434889999,"d":"0.85"},{"$f":"VLOOKUP(A47039,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.832248617,"d":"0.83"}]
["56033","56","WY","033","Sheridan","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",650.6404205417999,"A","CEC Survey",2017,15,"I",550.6999981929349,"TON",8,{"v":0.8463968434889999,"d":"0.85"},{"$f":"VLOOKUP(A47040,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.832248617,"d":"0.83"}]
["56033","56","WY","033","Sheridan","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",444.3397993944,"A","CEC Survey",2017,15,"I",376.08780364395557,"TON",8,{"v":0.8463968434889998,"d":"0.85"},{"$f":"VLOOKUP(A47041,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.8322486169999999,"d":"0.83"}]
["56035","56","WY","035","Sublette","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",83.39588386825679,"A","CEC Survey",2017,15,"I",155.22617622084098,"TON",8,{"v":1.861316998163325,"d":"1.86"},{"$f":"VLOOKUP(A47042,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":1.8284056956417731,"d":"1.83"}]
["56035","56","WY","035","Sublette","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.76182842175055,"A","CEC Survey",2017,15,"I",12.585906180068188,"TON",8,{"$f":"P47043/J47043","v":{"v":1.8613169981633249,"d":"1.86"}},{"$f":"VLOOKUP(A47043,cordwood_density!A:D,4,FALSE)","v":1.018},{"$f":"S47043/T47043","v":{"v":1.828405695641773,"d":"1.83"}}]
["56035","56","WY","035","Sublette","","2104008610","Hydronic heater: outdoor","Hydronic heater",81.1419410610066,"A","CEC Survey",2017,15,"I",151.03087416081823,"TON",8,{"v":1.8613169981633246,"d":"1.86"},{"$f":"VLOOKUP(A47044,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":1.8284056956417727,"d":"1.83"}]
["56035","56","WY","035","Sublette","","2104008620","Hydronic heater: indoor","Hydronic heater",51.84068456675422,"A","CEC Survey",2017,15,"I",96.49194738052277,"TON",8,{"v":1.861316998163325,"d":"1.86"},{"$f":"VLOOKUP(A47045,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":1.8284056956417731,"d":"1.83"}]
["56035","56","WY","035","Sublette","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.2539428072501835,"A","CEC Survey",2017,15,"I",4.195302060022729,"TON",8,{"v":1.8613169981633249,"d":"1.86"},{"$f":"VLOOKUP(A47046,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":1.828405695641773,"d":"1.83"}]
["56035","56","WY","035","Sublette","","2104008100","Fireplace: general","Fireplace: general",187.608866842,"A","CEC Survey",2017,15,"I",50.062133209906634,"TON",8,{"v":0.26684310849799997,"d":"0.27"},{"$f":"VLOOKUP(A47047,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":0.262124861,"d":"0.26"}]
["56035","56","WY","035","Sublette","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",57.92194741057,"A","CEC Survey",2017,15,"I",14.764274599672857,"TON",8,{"v":0.254899485596,"d":"0.25"},{"$f":"VLOOKUP(A47048,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":0.250392422,"d":"0.25"}]
["56035","56","WY","035","Sublette","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",76.60644657527,"A","CEC Survey",2017,15,"I",19.526943825373777,"TON",8,{"v":0.254899485596,"d":"0.25"},{"$f":"VLOOKUP(A47049,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":0.250392422,"d":"0.25"}]
["56035","56","WY","035","Sublette","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",52.31659766116,"A","CEC Survey",2017,15,"I",13.335473831962583,"TON",8,{"v":0.254899485596,"d":"0.25"},{"$f":"VLOOKUP(A47050,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":0.250392422,"d":"0.25"}]
["56035","56","WY","035","Sublette","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,507.963375864,"A","CEC Survey",2017,15,"I",88.78741819452624,"TON",8,{"v":0.17479098378599997,"d":"0.17"},{"$f":"VLOOKUP(A47051,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":0.17170037699999996,"d":"0.17"}]
["56035","56","WY","035","Sublette","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",157.72260750200002,"A","CEC Survey",2017,15,"I",117.94853546804859,"TON",8,{"v":0.747822632,"d":"0.75"},{"$f":"VLOOKUP(A47052,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":0.7345998349705304,"d":"0.73"}]
["56035","56","WY","035","Sublette","","2104009000","Wax Log; Total: All Combustor Types",null,60.53955500587012,"A","CEC Survey",2017,15,"I",47.25078366057359,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47053,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":0.766693909626719,"d":"0.77"}]
["56035","56","WY","035","Sublette","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",218.20063019933002,"A","CEC Survey",2017,15,"I",223.20712818573455,"TON",8,{"v":1.0229444707920001,"d":"1.02"},{"$f":"VLOOKUP(A47054,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":1.0048570440000002,"d":"1.00"}]
["56035","56","WY","035","Sublette","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",288.58793026363,"A","CEC Survey",2017,15,"I",295.2094276004876,"TON",8,{"v":1.022944470792,"d":"1.02"},{"$f":"VLOOKUP(A47055,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":1.004857044,"d":"1.00"}]
["56035","56","WY","035","Sublette","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",197.08444018004005,"A","CEC Survey",2017,15,"I",201.60643836130865,"TON",8,{"v":1.022944470792,"d":"1.02"},{"$f":"VLOOKUP(A47056,cordwood_density!A:D,4,FALSE)","v":1.018},{"v":1.004857044,"d":"1.00"}]
["56037","56","WY","037","Sweetwater","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",105.5231549590874,"A","CEC Survey",2017,15,"I",187.58223583691577,"TON",8,{"v":1.7776405179473989,"d":"1.78"},{"$f":"VLOOKUP(A47057,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7298954047755923,"d":"1.73"}]
["56037","56","WY","037","Sweetwater","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",8.555931483169248,"A","CEC Survey",2017,15,"I",15.20937047326344,"TON",8,{"v":1.777640517947399,"d":"1.78"},{"$f":"VLOOKUP(A47058,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7298954047755926,"d":"1.73"}]
["56037","56","WY","037","Sweetwater","","2104008610","Hydronic heater: outdoor","Hydronic heater",102.67117779803098,"A","CEC Survey",2017,15,"I",182.5124456791613,"TON",8,{"v":1.777640517947399,"d":"1.78"},{"$f":"VLOOKUP(A47059,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7298954047755926,"d":"1.73"}]
["56037","56","WY","037","Sweetwater","","2104008620","Hydronic heater: indoor","Hydronic heater",65.59547470429757,"A","CEC Survey",2017,15,"I",116.60517362835306,"TON",8,{"v":1.777640517947399,"d":"1.78"},{"$f":"VLOOKUP(A47060,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7298954047755926,"d":"1.73"}]
["56037","56","WY","037","Sweetwater","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.8519771610564164,"A","CEC Survey",2017,15,"I",5.069790157754481,"TON",8,{"v":1.777640517947399,"d":"1.78"},{"$f":"VLOOKUP(A47061,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7298954047755926,"d":"1.73"}]
["56037","56","WY","037","Sweetwater","","2104008100","Fireplace: general","Fireplace: general",1328.0039634510001,"A","CEC Survey",2017,15,"I",290.0853707448825,"TON",8,{"v":0.21843712724400002,"d":"0.22"},{"$f":"VLOOKUP(A47062,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.21257019000000002,"d":"0.21"}]
["56037","56","WY","037","Sweetwater","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",153.48368737977,"A","CEC Survey",2017,15,"I",33.11264829971932,"TON",8,{"v":0.21574050548959997,"d":"0.22"},{"$f":"VLOOKUP(A47063,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.20994599599999997,"d":"0.21"}]
["56037","56","WY","037","Sweetwater","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",202.99455427646998,"A","CEC Survey",2017,15,"I",43.79414775124168,"TON",8,{"v":0.21574050548960003,"d":"0.22"},{"$f":"VLOOKUP(A47064,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.20994599600000002,"d":"0.21"}]
["56037","56","WY","037","Sweetwater","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",138.63042731076,"A","CEC Survey",2017,15,"I",29.908198464262615,"TON",8,{"v":0.2157405054896,"d":"0.22"},{"$f":"VLOOKUP(A47065,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.209945996,"d":"0.21"}]
["56037","56","WY","037","Sweetwater","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1790.306551836,"A","CEC Survey",2017,15,"I",312.5708174614955,"TON",8,{"v":0.17459066836400003,"d":"0.17"},{"$f":"VLOOKUP(A47066,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.16990139,"d":"0.17"}]
["56037","56","WY","037","Sweetwater","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",382.97053548599996,"A","CEC Survey",2017,15,"I",123.81216668045725,"TON",8,{"v":0.323294236,"d":"0.32"},{"$f":"VLOOKUP(A47067,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.3146109731413001,"d":"0.31"}]
["56037","56","WY","037","Sweetwater","","2104009000","Wax Log; Total: All Combustor Types",null,308.0757023429781,"A","CEC Survey",2017,15,"I",240.45136045476127,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47068,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["56037","56","WY","037","Sweetwater","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",409.13590034426994,"A","CEC Survey",2017,15,"I",327.4806093018731,"TON",8,{"v":0.8004201269707999,"d":"0.80"},{"$f":"VLOOKUP(A47069,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7789218829999999,"d":"0.78"}]
["56037","56","WY","037","Sweetwater","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",541.11522303597,"A","CEC Survey",2017,15,"I",433.1195155282837,"TON",8,{"v":0.8004201269707998,"d":"0.80"},{"$f":"VLOOKUP(A47070,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7789218829999998,"d":"0.78"}]
["56037","56","WY","037","Sweetwater","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",369.54210353676,"A","CEC Survey",2017,15,"I",295.7889374339499,"TON",8,{"v":0.8004201269707999,"d":"0.80"},{"$f":"VLOOKUP(A47071,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7789218829999999,"d":"0.78"}]
["56039","56","WY","039","Teton","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",234.54554921857843,"A","CEC Survey",2017,15,"I",470.47818654309464,"TON",8,{"v":2.0059139391498113,"d":"2.01"},{"$f":"VLOOKUP(A47072,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9723834209929316,"d":"1.97"}]
["56039","56","WY","039","Teton","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",19.01720669339825,"A","CEC Survey",2017,15,"I",38.14687998998065,"TON",8,{"v":2.0059139391498113,"d":"2.01"},{"$f":"VLOOKUP(A47073,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9723834209929316,"d":"1.97"}]
["56039","56","WY","039","Teton","","2104008610","Hydronic heater: outdoor","Hydronic heater",228.206480320779,"A","CEC Survey",2017,15,"I",457.7625598797677,"TON",8,{"v":2.0059139391498113,"d":"2.01"},{"$f":"VLOOKUP(A47074,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9723834209929316,"d":"1.97"}]
["56039","56","WY","039","Teton","","2104008620","Hydronic heater: indoor","Hydronic heater",145.7985846493866,"A","CEC Survey",2017,15,"I",292.4594132565183,"TON",8,{"v":2.0059139391498113,"d":"2.01"},{"$f":"VLOOKUP(A47075,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9723834209929316,"d":"1.97"}]
["56039","56","WY","039","Teton","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",6.339068897799417,"A","CEC Survey",2017,15,"I",12.715626663326882,"TON",8,{"v":2.0059139391498113,"d":"2.01"},{"$f":"VLOOKUP(A47076,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.9723834209929316,"d":"1.97"}]
["56039","56","WY","039","Teton","","2104008100","Fireplace: general","Fireplace: general",508.336796075,"A","CEC Survey",2017,15,"I",110.85942404892536,"TON",8,{"v":0.21808262731499997,"d":"0.22"},{"$f":"VLOOKUP(A47077,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.214437195,"d":"0.21"}]
["56039","56","WY","039","Teton","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",153.1564965756,"A","CEC Survey",2017,15,"I",51.342963709141756,"TON",8,{"v":0.335232032967,"d":"0.34"},{"$f":"VLOOKUP(A47078,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.32962835100000004,"d":"0.33"}]
["56039","56","WY","039","Teton","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",202.5618180516,"A","CEC Survey",2017,15,"I",67.90521006692941,"TON",8,{"v":0.33523203296699994,"d":"0.34"},{"$f":"VLOOKUP(A47079,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.329628351,"d":"0.33"}]
["56039","56","WY","039","Teton","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",138.33490013280002,"A","CEC Survey",2017,15,"I",46.37428980180546,"TON",8,{"v":0.33523203296699994,"d":"0.34"},{"$f":"VLOOKUP(A47080,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.329628351,"d":"0.33"}]
["56039","56","WY","039","Teton","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,1075.073597065,"A","CEC Survey",2017,15,"I",184.40337514469982,"TON",8,{"v":0.17152628029199996,"d":"0.17"},{"$f":"VLOOKUP(A47081,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.16865907599999996,"d":"0.17"}]
["56039","56","WY","039","Teton","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",271.073465425,"A","CEC Survey",2017,15,"I",368.65205049213534,"TON",8,{"v":1.359970995,"d":"1.36"},{"$f":"VLOOKUP(A47082,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.3372379498525075,"d":"1.34"}]
["56039","56","WY","039","Teton","","2104009000","Wax Log; Total: All Combustor Types",null,166.54531944842904,"A","CEC Survey",2017,15,"I",129.98768917570993,"TON",8,{"v":0.7804943999999998,"d":"0.78"},{"$f":"VLOOKUP(A47083,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106194,"d":"0.77"}]
["56039","56","WY","039","Teton","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",515.7639069985499,"A","CEC Survey",2017,15,"I",507.07349084762865,"TON",8,{"v":0.9831503987910001,"d":"0.98"},{"$f":"VLOOKUP(A47084,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9667162230000002,"d":"0.97"}]
["56039","56","WY","039","Teton","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",682.1393608690499,"A","CEC Survey",2017,15,"I",670.6455846694444,"TON",8,{"v":0.9831503987910001,"d":"0.98"},{"$f":"VLOOKUP(A47085,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9667162230000002,"d":"0.97"}]
["56039","56","WY","039","Teton","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",465.8512708374,"A","CEC Survey",2017,15,"I",458.001862701084,"TON",8,{"v":0.9831503987910001,"d":"0.98"},{"$f":"VLOOKUP(A47086,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.9667162230000002,"d":"0.97"}]
["56041","56","WY","041","Uinta","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",80.3332374403251,"A","CEC Survey",2017,15,"I",146.69698167689876,"TON",8,{"v":1.826105686153523,"d":"1.83"},{"$f":"VLOOKUP(A47087,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":1.8078464371384249,"d":"1.81"}]
["56041","56","WY","041","Uinta","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",6.513505738404738,"A","CEC Survey",2017,15,"I",11.894349865694494,"TON",8,{"v":1.8261056861535232,"d":"1.83"},{"$f":"VLOOKUP(A47088,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":1.807846437138425,"d":"1.81"}]
["56041","56","WY","041","Uinta","","2104008610","Hydronic heater: outdoor","Hydronic heater",78.16206886085686,"A","CEC Survey",2017,15,"I",142.73219838833393,"TON",8,{"v":1.826105686153523,"d":"1.83"},{"$f":"VLOOKUP(A47089,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":1.8078464371384249,"d":"1.81"}]
["56041","56","WY","041","Uinta","","2104008620","Hydronic heater: indoor","Hydronic heater",49.936877327769665,"A","CEC Survey",2017,15,"I",91.19001563699112,"TON",8,{"v":1.8261056861535228,"d":"1.83"},{"$f":"VLOOKUP(A47090,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":1.8078464371384246,"d":"1.81"}]
["56041","56","WY","041","Uinta","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",2.171168579468246,"A","CEC Survey",2017,15,"I",3.9647832885648313,"TON",8,{"v":1.826105686153523,"d":"1.83"},{"$f":"VLOOKUP(A47091,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":1.8078464371384249,"d":"1.81"}]
["56041","56","WY","041","Uinta","","2104008100","Fireplace: general","Fireplace: general",512.36804542,"A","CEC Survey",2017,15,"I",116.5022688844104,"TON",8,{"v":0.22738004433689998,"d":"0.23"},{"$f":"VLOOKUP(A47092,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.22510646899999998,"d":"0.23"}]
["56041","56","WY","041","Uinta","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",88.21673992335,"A","CEC Survey",2017,15,"I",19.342535962054285,"TON",8,{"v":0.2192615140716,"d":"0.22"},{"$f":"VLOOKUP(A47093,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.217069116,"d":"0.22"}]
["56041","56","WY","041","Uinta","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",116.67375280185,"A","CEC Survey",2017,15,"I",25.582063691749212,"TON",8,{"v":0.2192615140716,"d":"0.22"},{"$f":"VLOOKUP(A47094,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.217069116,"d":"0.22"}]
["56041","56","WY","041","Uinta","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",79.6796360598,"A","CEC Survey",2017,15,"I",17.470677643145805,"TON",8,{"v":0.2192615140716,"d":"0.22"},{"$f":"VLOOKUP(A47095,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.217069116,"d":"0.22"}]
["56041","56","WY","041","Uinta","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,869.06746071,"A","CEC Survey",2017,15,"I",150.4652193183611,"TON",8,{"v":0.17313410767380003,"d":"0.17"},{"$f":"VLOOKUP(A47096,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.17140293800000003,"d":"0.17"}]
["56041","56","WY","041","Uinta","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",212.406994215,"A","CEC Survey",2017,15,"I",100.86995472147042,"TON",8,{"v":0.474889987,"d":"0.47"},{"$f":"VLOOKUP(A47097,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.47014155727155726,"d":"0.47"}]
["56041","56","WY","041","Uinta","","2104009000","Wax Log; Total: All Combustor Types",null,145.90468292781648,"A","CEC Survey",2017,15,"I",113.87778795893635,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47098,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.7726902286902286,"d":"0.77"}]
["56041","56","WY","041","Uinta","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",268.42663674755,"A","CEC Survey",2017,15,"I",241.57292502282618,"TON",8,{"v":0.8999588414544001,"d":"0.90"},{"$f":"VLOOKUP(A47099,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.8909601440000001,"d":"0.89"}]
["56041","56","WY","041","Uinta","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",355.01587440804997,"A","CEC Survey",2017,15,"I",319.49967503018945,"TON",8,{"v":0.8999588414544001,"d":"0.90"},{"$f":"VLOOKUP(A47100,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.8909601440000001,"d":"0.89"}]
["56041","56","WY","041","Uinta","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",242.44986544940002,"A","CEC Survey",2017,15,"I",218.1949000206172,"TON",8,{"v":0.8999588414544,"d":"0.90"},{"$f":"VLOOKUP(A47101,cordwood_density!A:D,4,FALSE)","v":1.0101},{"v":0.890960144,"d":"0.89"}]
["56043","56","WY","043","Washakie","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",35.932461939712,"A","CEC Survey",2017,15,"I",63.91516985137361,"TON",8,{"v":1.7787584373876582,"d":"1.78"},{"$f":"VLOOKUP(A47102,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7309832983531122,"d":"1.73"}]
["56043","56","WY","043","Washakie","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",2.913442859976649,"A","CEC Survey",2017,15,"I",5.182311069030293,"TON",8,{"v":1.778758437387658,"d":"1.78"},{"$f":"VLOOKUP(A47103,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.730983298353112,"d":"1.73"}]
["56043","56","WY","043","Washakie","","2104008610","Hydronic heater: outdoor","Hydronic heater",34.96131431971978,"A","CEC Survey",2017,15,"I",62.187732828363515,"TON",8,{"v":1.7787584373876582,"d":"1.78"},{"$f":"VLOOKUP(A47104,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.7309832983531122,"d":"1.73"}]
["56043","56","WY","043","Washakie","","2104008620","Hydronic heater: indoor","Hydronic heater",22.336395259820975,"A","CEC Survey",2017,15,"I",39.731051529232246,"TON",8,{"v":1.778758437387658,"d":"1.78"},{"$f":"VLOOKUP(A47105,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.730983298353112,"d":"1.73"}]
["56043","56","WY","043","Washakie","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",0.9711476199922163,"A","CEC Survey",2017,15,"I",1.7274370230100977,"TON",8,{"v":1.778758437387658,"d":"1.78"},{"$f":"VLOOKUP(A47106,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":1.730983298353112,"d":"1.73"}]
["56043","56","WY","043","Washakie","","2104008100","Fireplace: general","Fireplace: general",275.32749251,"A","CEC Survey",2017,15,"I",65.50365130729487,"TON",8,{"$f":"P47107/J47107","v":{"v":0.23791177085200002,"d":"0.24"}},{"$f":"VLOOKUP(A47107,cordwood_density!A:D,4,FALSE)","v":1.0276},{"$f":"S47107/T47107","v":{"v":0.23152177000000002,"d":"0.23"}}]
["56043","56","WY","043","Washakie","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",43.3095345724,"A","CEC Survey",2017,15,"I",10.183532465827572,"TON",8,{"v":0.23513373132200002,"d":"0.24"},{"$f":"VLOOKUP(A47108,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.228818345,"d":"0.23"}]
["56043","56","WY","043","Washakie","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",57.28035217639999,"A","CEC Survey",2017,15,"I",13.468542938675176,"TON",8,{"v":0.23513373132200005,"d":"0.24"},{"$f":"VLOOKUP(A47109,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22881834500000003,"d":"0.23"}]
["56043","56","WY","043","Washakie","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",39.1182892912,"A","CEC Survey",2017,15,"I",9.198029323973293,"TON",8,{"v":0.23513373132200005,"d":"0.24"},{"$f":"VLOOKUP(A47110,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.22881834500000003,"d":"0.23"}]
["56043","56","WY","043","Washakie","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,468.94176881000004,"A","CEC Survey",2017,15,"I",82.53858277164777,"TON",8,{"v":0.176010302902,"d":"0.18"},{"$f":"VLOOKUP(A47111,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.171282895,"d":"0.17"}]
["56043","56","WY","043","Washakie","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",115.32843553,"A","CEC Survey",2017,15,"I",45.77290587087667,"TON",8,{"v":0.39689176100000007,"d":"0.40"},{"$f":"VLOOKUP(A47112,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.38623176430517714,"d":"0.39"}]
["56043","56","WY","043","Washakie","","2104009000","Wax Log; Total: All Combustor Types",null,66.08790959352102,"A","CEC Survey",2017,15,"I",51.58124334544943,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47113,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.7595313351498636,"d":"0.76"}]
["56043","56","WY","043","Washakie","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",125.09674202810001,"A","CEC Survey",2017,15,"I",107.05962833083518,"TON",8,{"v":0.8558146806636002,"d":"0.86"},{"$f":"VLOOKUP(A47114,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8328286110000002,"d":"0.83"}]
["56043","56","WY","043","Washakie","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",165.4505297791,"A","CEC Survey",2017,15,"I",141.59499230852396,"TON",8,{"v":0.8558146806636002,"d":"0.86"},{"$f":"VLOOKUP(A47115,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8328286110000002,"d":"0.83"}]
["56043","56","WY","043","Washakie","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",112.99060570280002,"A","CEC Survey",2017,15,"I",96.69901913752857,"TON",8,{"v":0.8558146806636002,"d":"0.86"},{"$f":"VLOOKUP(A47116,cordwood_density!A:D,4,FALSE)","v":1.0276},{"v":0.8328286110000002,"d":"0.83"}]
["56045","56","WY","045","Weston","","2104008510","Furnace: Indoor, cordwood-fired, non-EPA certified","Furnace",39.16810421643393,"A","CEC Survey",2017,15,"I",69.39124585453382,"TON",8,{"v":1.7716263588121028,"d":"1.77"},{"$f":"VLOOKUP(A47117,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7420121522242902,"d":"1.74"}]
["56045","56","WY","045","Weston","","2104008530","Furnace: Indoor, pellet-fired, general","Furnace-Pellet",3.1757922337649136,"A","CEC Survey",2017,15,"I",5.626317231448688,"TON",8,{"v":1.7716263588121026,"d":"1.77"},{"$f":"VLOOKUP(A47118,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.74201215222429,"d":"1.74"}]
["56045","56","WY","045","Weston","","2104008610","Hydronic heater: outdoor","Hydronic heater",38.10950680517896,"A","CEC Survey",2017,15,"I",67.51580677738426,"TON",8,{"v":1.7716263588121028,"d":"1.77"},{"$f":"VLOOKUP(A47119,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7420121522242902,"d":"1.74"}]
["56045","56","WY","045","Weston","","2104008620","Hydronic heater: indoor","Hydronic heater",24.34774045886434,"A","CEC Survey",2017,15,"I",43.135098774439946,"TON",8,{"v":1.7716263588121026,"d":"1.77"},{"$f":"VLOOKUP(A47120,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.74201215222429,"d":"1.74"}]
["56045","56","WY","045","Weston","","2104008630","Hydronic heater: pellet-fired","Pellet Hydronic Heater",1.0585974112549712,"A","CEC Survey",2017,15,"I",1.8754390771495628,"TON",8,{"v":1.7716263588121028,"d":"1.77"},{"$f":"VLOOKUP(A47121,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":1.7420121522242902,"d":"1.74"}]
["56045","56","WY","045","Weston","","2104008100","Fireplace: general","Fireplace: general",162.04140898,"A","CEC Survey",2017,15,"I",39.22461539749723,"TON",8,{"v":0.24206538096899996,"d":"0.24"},{"$f":"VLOOKUP(A47122,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.23801905699999998,"d":"0.24"}]
["56045","56","WY","045","Weston","","2104008210","Woodstove: fireplace inserts; non-EPA certified","Woodstove or Fireplace Insert",53.02268210806,"A","CEC Survey",2017,15,"I",12.01239769218607,"TON",8,{"v":0.22655205686699995,"d":"0.23"},{"$f":"VLOOKUP(A47123,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.22276505099999996,"d":"0.22"}]
["56045","56","WY","045","Weston","","2104008220","Woodstove: fireplace inserts; EPA certified; non-catalytic","Woodstove or Fireplace Insert",70.12677311066,"A","CEC Survey",2017,15,"I",15.887364689665446,"TON",8,{"v":0.22655205686699995,"d":"0.23"},{"$f":"VLOOKUP(A47124,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.22276505099999996,"d":"0.22"}]
["56045","56","WY","045","Weston","","2104008230","Woodstove: fireplace inserts; EPA certified; catalytic","Woodstove or Fireplace Insert",47.891454807280006,"A","CEC Survey",2017,15,"I",10.849907592942259,"TON",8,{"v":0.22655205686699997,"d":"0.23"},{"$f":"VLOOKUP(A47125,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.222765051,"d":"0.22"}]
["56045","56","WY","045","Weston","","2104008700","Outdoor wood burning device, NEC (fire-pits, chimeas, etc)",null,430.705547612,"A","CEC Survey",2017,15,"I",75.09527840273235,"TON",8,{"v":0.17435410065899998,"d":"0.17"},{"$f":"VLOOKUP(A47126,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.17143962699999998,"d":"0.17"}]
["56045","56","WY","045","Weston","","2104008400","Woodstove: pellet-fired, general","Pellet Woodstove",113.08791407,"A","CEC Survey",2017,15,"I",52.23318202158806,"TON",8,{"v":0.461881205,"d":"0.46"},{"$f":"VLOOKUP(A47127,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.4541604768928221,"d":"0.45"}]
["56045","56","WY","045","Weston","","2104009000","Wax Log; Total: All Combustor Types",null,60.25550954916444,"A","CEC Survey",2017,15,"I",47.029087772269364,"TON",8,{"v":0.7804943999999999,"d":"0.78"},{"$f":"VLOOKUP(A47128,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.7674477876106195,"d":"0.77"}]
["56045","56","WY","045","Weston","","2104008310","Woodstove: freestanding; non-EPA certified","Woodstove or Fireplace Insert",150.21681877774,"A","CEC Survey",2017,15,"I",133.93867951813112,"TON",8,{"v":0.8916357076920001,"d":"0.89"},{"$f":"VLOOKUP(A47129,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.8767312760000001,"d":"0.88"}]
["56045","56","WY","045","Weston","","2104008320","Woodstove: freestanding; EPA certified; non-catalytic","Woodstove or Fireplace Insert",198.67385709314,"A","CEC Survey",2017,15,"I",177.14470516914113,"TON",8,{"v":0.891635707692,"d":"0.89"},{"$f":"VLOOKUP(A47130,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.876731276,"d":"0.88"}]
["56045","56","WY","045","Weston","","2104008330","Woodstove: freestanding; EPA certified; catalytic","Woodstove or Fireplace Insert",135.67970728312002,"A","CEC Survey",2017,15,"I",120.97687182282812,"TON",8,{"v":0.891635707692,"d":"0.89"},{"$f":"VLOOKUP(A47131,cordwood_density!A:D,4,FALSE)","v":1.017},{"v":0.876731276,"d":"0.88"}]