{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["factor summary","data included","data excluded"],"read":"whole","date_system":"1900"}

{"sheet":"factor summary","index":0,"n_rows":15,"n_cols":2,"rows_kept":15}
["Key Parameters","Results"]
["SCC",10200902]
["Does the SCC contain more than 15 sources?","Yes"]
["Pollutant","CARBON MONOXIDE"]
["Units","LB"]
["Activity","MILLION BTUS HEAT INPUT"]
["Factor Quality Rating","Highly"]
["Number of individual test data values used to calculate the emissions factor",34]
["Number of individual test data values excluded from the calculation",1]
["Composite Test Rating",78.14]
["Control Device Configuration","UNCONTROLLED"]
["Existing Factor",{"v":0.6,"d":"6.00E-01"}]
["New Candidate Factor Value ",{"v":0.75,"d":"7.50E-01"}]
["Difference (%)",25.01]
["AP42 Section",1.6]

{"sheet":"data included","index":1,"n_rows":35,"n_cols":11,"rows_kept":35}
["Test Data Value","Individual Test Method","Individual Test Data Units","Individual Test Data Activity","Individual Test Rating","Detection Limit Flag ","Year of Test","Facility Name","Test City","Test State","ERT Project Dataset"]
[0.087,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"Hood Industries - Metcalfe","Metcalf","GA","PDS"]
[0.829,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]
[0.771,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Hood Industries Waynesboro Sawmill","Waynesboro","MS","PDS"]
[0.763,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]
[0.694,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]
[0.643,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"Hood Industries INC, Wiggins","Wiggins","MS","PDS"]
[0.575,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Hood Industries-Wiggins Plywood Plant","Wiggins","MS","PDS"]
[0.0472,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]
[0.418,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Hood-Metcalfe Sawmill","Metcalfe","GA","PDS"]
[0.353,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Hood Industries Metcalf Sawmill","Metcalf","GA","PDS"]
[0.343,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Hood Industries-Wiggins Plywood Plant","Wiggins","MS","PDS"]
[0.28,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Hood Industries Metcalf Sawmill","Metcalf","GA","PDS"]
[2.77,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Hood Industries-Wiggins Plywood Plant","Wiggins","MS","PDS"]
[2.73,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Hood Industries Wiggins Plywood Plant","Wiggins","MS","PDS"]
[0.264,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]
[0.243,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"Hood Industries - Metcalfe","Metcalf","GA","PDS"]
[0.237,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Hood Industries Metcalf Sawmill","Metcalf","GA","PDS"]
[0.225,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Hood Industries Metcalf Sawmill","Metcalf","GA","PDS"]
[0.198,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Hood Industries Metcalf Sawmill","Metcalf","GA","PDS"]
[0.186,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]
[1.74,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Hood Industries-Wiggins Plywood Plant","Wiggins","MS","PDS"]
[1.64,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Hood-Wiggins","Wiggins","MS","PDS"]
[0.155,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Hood Industries Metcalfe Sawmill","Metcalf","GA","PDS"]
[1.55,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Hood Industries-Wiggins Plywood Plant","Wiggins","MS","PDS"]
[0.151,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Hood Industries Metcalf Sawmill","Metcalf","GA","PDS"]
[1.49,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2015,"Hood Industries Waynesboro Sawmill","Waynesboro","MS","PDS"]
[1.46,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Hunt Forest Products-Pollock Plywood Plant","Pollock","LA","PDS"]
[1.38,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Hunt Forest Products-Pollock Plywood Plant","Pollock","LA","PDS"]
[0.135,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Hood Industries Metcalf Sawmill","Metcalf","GA","PDS"]
[1.19,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"Hood Industries INC, Wiggins","Wiggins","MS","PDS"]
[1.1,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"Hood Industries Inc.","Waynesboro","MS","PDS"]
[0.107,"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2015,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]
[0.0187,"Method 10","LB","MILLION BTUS HEAT INPUT",74,"ADL",2020,"Interational Paper Savannah","Savannah","GA","PDS"]
[0.721,"Method 10","LB","MILLION BTUS HEAT INPUT",72,"ADL",2018,"Rayonier Performance Fibers, LLC","Jesup","GA","PDS"]

{"sheet":"data excluded","index":2,"n_rows":2,"n_cols":12,"rows_kept":2}
["Reason for Exclusion","Test Data Value","Individual Test Method","Individual Test Data Units","Individual Test Data Activity","Individual Test Rating","Detection Limit Flag ","Year of Test","Facility Name","Test City","Test State","ERT Project Dataset"]
["EPA Manually Excluded - Duplicate",{"v":0.107,"d":"1.07E-01"},"Method 10","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2015,"T.R. Miller Mill Company, Inc.","Brewton","AL","PDS"]