{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["factor summary","data included","data excluded"],"read":"whole","date_system":"1900"}

{"sheet":"factor summary","index":0,"n_rows":13,"n_cols":2,"rows_kept":13}
["Key Parameters","Results"]
["SCC",10200902]
["Does the SCC contain more than 15 sources?","Yes"]
["Pollutant","PM, FILTERABLE"]
["Units","LB"]
["Activity","MILLION BTUS HEAT INPUT"]
["Factor Quality Rating","Highly"]
["Number of individual test data values used to calculate the emissions factor",48]
["Number of individual test data values excluded from the calculation",7]
["Composite Test Rating",77.39]
["Control Device Configuration","ELECTROSTATIC PRECIPITATOR"]
["New Candidate Factor Value ",{"v":0.0125,"d":"1.25E-02"}]
["AP42 Section",1.6]

{"sheet":"data included","index":1,"n_rows":49,"n_cols":11,"rows_kept":49}
["Individual Test Data Value","Individual Test Method","Individual Test Data Units","Individual Test Data Activity","Individual Test Rating","Detection Limit Flag ","Year of Test","Facility Name","Test City","Test State","ERT Project Dataset"]
[{"v":5.14e-05,"d":"5.14E-05"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"Boise Cascade Wood Products, LLC, Elgin Complex","Elgin","OR","PDS"]
[{"v":1.35E-4,"d":"1.35E-04"},"Method 5","LB","MILLION BTUS HEAT INPUT",72,"ADL",2016,"Boise Cascade Wood Products, LLC, Elgin Complex","Elgin","OR","PDS"]
[{"v":0.000625,"d":"6.25E-04"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"DLL",2017,"Georgia-Pacific Consumer Products (Camas), LLC","Camas","WA","PDS"]
[{"v":1.06E-3,"d":"1.06E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Georgia-Pacific Consumer Products (Camas), LLC","Camas","WA","PDS"]
[{"v":0.00118,"d":"1.18E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",77.5,"ADL",2016,"The Westervelt Compay","Moundville","AL","PDS"]
[{"v":0.00122,"d":"1.22E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"The Westervelt Company","Moundville","AL","PDS"]
[{"v":0.00137,"d":"1.37E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"The Westervelt Compay","Moundville","AL","PDS"]
[{"v":1.42E-3,"d":"1.42E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",74.5,"ADL",2019,"IP- Port Wentworth","Port Wentworth","GA","PDS"]
[{"v":1.47E-3,"d":"1.47E-03"},"Method 5/26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"Domtar Paper Company, LLC","Hawesville","KY","PDS"]
[{"v":0.00194,"d":"1.94E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"DLL",2019,"Weyerhaeuser Raymond Lumber Mill","Raymond","WA","PDS"]
[{"v":1.97E-3,"d":"1.97E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"The Westervelt Company","Moundville","AL","PDS"]
[{"v":0.00203,"d":"2.03E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",77.5,"ADL",2019,"The Westervelt Company","Moundville","AL","PDS"]
[{"v":0.00236,"d":"2.36E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"The Westervelt Compay","Moundville","AL","PDS"]
[{"v":0.0024,"d":"2.40E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"The Westervelt Compay","Moundville","AL","PDS"]
[{"v":2.63E-3,"d":"2.63E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Mannington Wood Floors","Epes","AL","PDS"]
[{"v":0.0027,"d":"2.70E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",77.5,"ADL",2016,"The Westervelt Compay","Moundville","AL","PDS"]
[{"v":0.00324,"d":"3.24E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Roseburg Forest Products Coquille Plywood","Coquille","OR","PDS"]
[{"v":0.00343,"d":"3.43E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"The Westervelt Company","Moundville","AL","PDS"]
[{"v":0.00386,"d":"3.86E-03"},"Method 5/26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Domtar Paper Company, LLC","Hawesville","KY","PDS"]
[{"v":0.0039,"d":"3.90E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"The Westervelt Compay","Moundville","AL","PDS"]
[{"v":3.98E-3,"d":"3.98E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Verso Quinnesec LLC","Quinnesec","MI","PDS"]
[{"v":0.0041,"d":"4.10E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Domtar Paper Company, LLC","Bennettsville","SC","PDS"]
[{"v":0.00456,"d":"4.56E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Interfor U.S. Inc.","Perry","GA","PDS"]
[{"v":0.00523,"d":"5.23E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",80,"ADL",2017,"Georgia-Pacific Consumer Operations LLC","Palatka","FL","PDS"]
[{"v":0.00581,"d":"5.81E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"Verso Quinnesec LLC","Quinnesec","MI","PDS"]
[{"v":0.00592,"d":"5.92E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",72.5,"ADL",2018,"IP- Port Wentworth","Port Wentworth","GA","PDS"]
[{"v":0.00593,"d":"5.93E-03"},"Method 5/26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Domtar Paper Company, LLC","Hawesville","KY","PDS"]
[{"v":0.00635,"d":"6.35E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Domtar Paper Company, LLC","Bennettsville","SC","PDS"]
[{"v":0.00741,"d":"7.41E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",80,"ADL",2018,"Georgia-Pacific Consumer Operations LLC","Palatka","FL","PDS"]
[{"v":0.00766,"d":"7.66E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",75,"ADL",2017,"Georgia Pacific Alabama River Cellulose","Perdue Hill","AL","PDS"]
[{"v":0.00825,"d":"8.25E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",77.5,"ADL",2020,"Domtar Paper Company, LLC","Bennettsville","SC","PDS"]
[{"v":0.00986,"d":"9.86E-03"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Interfor U.S. Inc. - Perry Mill","Perry","GA","PDS"]
[{"v":0.0114,"d":"1.14E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"Interfor U.S. Inc. - Perry Mill","Perry","GA","PDS"]
[{"v":0.0128,"d":"1.28E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",77.5,"ADL",2016,"International Paper - Augusta Mill","Augusta","GA","PDS"]
[{"v":0.0128,"d":"1.28E-02"},"Method 5","LB","MILLION BTUS HEAT INPUT",77.5,"ADL",2019,"Interfor U.S. Inc. Baxley Sawmill","Baxley","GA","PDS"]
[{"v":0.0152,"d":"1.52E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2016,"Georgia-Pacific Consumer Products (Camas), LLC","Camas","WA","PDS"]
[0.0158,"Method 5","LB","MILLION BTUS HEAT INPUT",65,"ADL",2020,"Georgia-Pacific Monticello LLC","Monticello","MS","PDS"]
[{"v":0.018,"d":"1.80E-02"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"Georgia Pacific Alabama River Cellulose","Perdue Hill","AL","PDS"]
[{"v":0.0212,"d":"2.12E-02"},"Method 5","LB","MILLION BTUS HEAT INPUT",78,"ADL",2019,"Interfor U.S. Inc. Baxley Sawmill","Baxley","GA","PDS"]
[{"v":0.0223,"d":"2.23E-02"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2020,"Georgia-Pacific Monticello LLC","Monticello","MS","PDS"]
[{"v":0.0254,"d":"2.54E-02"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2015,"Boise Cascade Wood Products, LLC, Elgin Complex","Elgin","OR","PDS"]
[{"v":0.026,"d":"2.60E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Mannington Wood Floors","Epes","AL","PDS"]
[{"v":0.0267,"d":"2.67E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2019,"Canfor Southern Pine - Graham Plant","Graham","NC","PDS"]
[{"v":0.0289,"d":"2.89E-02"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Interfor U.S. Inc. Baxley Sawmill","Baxley","GA","PDS"]
[{"v":0.0307,"d":"3.07E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",69,"ADL",2016,"Georgia-Pacific Consumer Operations LLC","Palatka","FL","PDS"]
[{"v":0.0347,"d":"3.47E-02"},"Method 5","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2018,"Interfor U.S. Inc. Baxley Sawmill","Baxley","GA","PDS"]
[{"v":0.0529,"d":"5.29E-02"},"Method 29","LB","MILLION BTUS HEAT INPUT",79,"ADL",2020,"SAPPI Somerset Mill","Skowhegan","ME","PDS"]
[{"v":0.133,"d":"1.33E-01"},"Method 5","LB","MILLION BTUS HEAT INPUT",79,"ADL",2020,"SAPPI Somerset Mill","Skowhegan","ME","PDS"]

{"sheet":"data excluded","index":2,"n_rows":8,"n_cols":12,"rows_kept":8}
["Reason for Exclusion","Individual Test Data Value","Individual Test Method","Individual Test Data Units","Individual Test Data Activity","Individual Test Rating","Detection Limit Flag ","Year of Test","Facility Name","Test City","Test State","ERT Project Data Set"]
["Data value does not improve the factor quality rating.",{"v":0.00505,"d":"5.05E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",27,"ADL",2016,"Georgia Pacific Alabama River Cellulose","Perdue Hill","AL","PDS"]
["Data value does not improve the factor quality rating.",{"v":0.000277,"d":"2.77E-04"},"Method 5","LB","MILLION BTUS HEAT INPUT",22.5,"ADL",2017,"WestRock CP, LLC","West Point","VA","PDS"]
["Data value does not improve the factor quality rating.",{"v":0.000225,"d":"2.25E-04"},"Method 5","LB","MILLION BTUS HEAT INPUT",22.5,"ADL",2016,"WestRock CP, LLC","West Point","VA","PDS"]
["Data value does not improve the factor quality rating.",{"v":0.00186,"d":"1.86E-03"},"Method 5","LB","MILLION BTUS HEAT INPUT",22.5,"ADL",2018,"WestRock CP, LLC","West Point","VA","PDS"]
["EPA Manually Excluded - Duplicate",{"v":0.0024,"d":"2.40E-03"},"Method 5/202","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"The Westervelt Compay","Moundville","AL","PDS"]
["EPA Manually Excluded - Duplicate",{"v":0.0307,"d":"3.07E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",69,"ADL",2016,"Georgia-Pacific Consumer Operations LLC","Palatka","FL","PDS"]
["EPA Manually Excluded - Duplicate",{"v":0.026,"d":"2.60E-02"},"Method 26A","LB","MILLION BTUS HEAT INPUT",78.5,"ADL",2017,"Mannington Wood Floors","Epes","AL","PDS"]