{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Family Info","ESRI_MAPINFO_SHEET"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Family Info","index":0,"n_rows":53550,"n_cols":43,"rows_kept":2250,"cut":true,"bounds":{"rows_first":1000,"rows_last":250,"rows_between":1000,"halvings":1}}
[]
["Model Year","Manufacturer Name","Engine Family/Testgroup","Evaporative Family","Represented Test Vehicle Make","Represented Test Vehicle Model","Vehicle ID","Vehicle Configuration Number","Displacement (L)","Curb Weight (lbs.)","Gross Vehicle Weight Rating (lbs.)","Equivalent Test Weight (lbs.)","Drive System","Drive System Description","Transmission Type","Transmission Type Description","Transmission type, if other","Number of Gears","Transmission Lockup Yes/No?","Creeper Gear Yes/No?","Vehicle Fuel Category","Vehicle Fuel Category Description","Hybrid Yes/No?","Test Number","Test Originator","Test Procedure","Test Procedure Description","Test Fuel","Test Fuel Description","Certification/In-Use Code","Deterioration Factor Type","Deterioration Factor Type Description","Certification Region","Certification Region Description","Standard Level","Standard Level Description","Useful Life Miles (k)","Emission Name","Rounded Emission Result (g/mi)","Certification Level (g/mi)","Emission Standard (g/mi)","Additive Deterioration Factor","Carline Models Covered"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10071584","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.11,0.1,"0.2",0.006,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10071584","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.11,0.1,"0.2",0.006,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10082351","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.007,0.01,"0.05",0,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10082351","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.007,0.01,"0.05",0,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10082352","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.279,0.281,"0.300",2.1000000000000003E-3,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10082352","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.279,0.281,"0.300",2.1000000000000003E-3,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071437","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071437","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071438","MFR","66","Leak Test - Evap Fuel System OBD","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.003,0,"0.02",0,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071438","MFR","66","Leak Test - Evap Fuel System OBD","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.003,0,"0.02",0,"Aston Martin Lagonda Ltd: DB12 V8, Vantage"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065519","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.02,0,"0.2",0.006,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065519","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.02,0,"0.2",0.006,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065539","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.26,0.26,"0.500",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065539","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.26,0.26,"0.500",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065541","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.366,0.366,"0.500",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065541","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.366,0.366,"0.500",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065542","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065542","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071437","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071437","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071438","MFR","66","Leak Test - Evap Fuel System OBD","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","3Z","California LEV-III Zero Evap (Option 1)","150","LEAK-DIA",0.003,0,"0.02",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXJ04.0AEX","SASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071438","MFR","66","Leak Test - Evap Fuel System OBD","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.003,0,"0.02",0,"Aston Martin Lagonda Ltd: DBX 707"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10071584","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.11,0.1,"0.2",6.3E-3,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10071584","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.11,0.1,"0.2",6.3E-3,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10082351","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.007,0.01,"0.05",0,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10082351","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.007,0.01,"0.05",0,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DB11 V8","564TT5477",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NASX10082352","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.279,0.281,"0.300",2.1000000000000003E-3,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071437","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071437","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071438","MFR","66","Leak Test - Evap Fuel System OBD","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.003,0,"0.02",0,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"aston martin","SASXV05.2AMV","SASXR0160T3A","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10071438","MFR","66","Leak Test - Evap Fuel System OBD","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.003,0,"0.02",0,"Aston Martin Lagonda Ltd: Vanquish"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.300",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.300",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.300",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.300",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.033,0.03,"0.20",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.033,0.03,"0.20",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4P","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.02",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 xDrive30i"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.041,0.04,"0.20",1E-3,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",1E-3,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ02.0B4X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.350",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.350",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.350",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.350",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.033,0.03,"0.20",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.033,0.03,"0.20",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.02",0,"BMW: 540i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075015","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3743,0.374,"0.500",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075015","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3743,0.374,"0.500",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075024","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3173,0.317,"0.500",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075024","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3173,0.317,"0.500",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075152","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.02,0.02,"0.05",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075152","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.02,0.02,"0.05",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075154","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075154","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075385","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075385","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.02",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075449","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.012700000000000001,0.013000000000000001,"0.020",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0180G0X","BMW","X7 xDrive40i","9K06067",0,3,5717,7088,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075449","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.012700000000000001,0.013000000000000001,"0.020",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075389","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24530000000000002,0.277,"0.400",0.0316,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075389","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24530000000000002,0.277,"0.400",0.0316,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075390","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24500000000000002,0.277,"0.400",0.0316,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075390","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24500000000000002,0.277,"0.400",0.0316,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075391","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.014,0.01,"0.05",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075391","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.014,0.01,"0.05",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075395","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.059000000000000004,0.06,"0.20",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075395","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.059000000000000004,0.06,"0.20",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075396","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.014,0.01,"0.02",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075396","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.014,0.01,"0.02",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075448","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0067,0.007,"0.020",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B58","SBMXR0190G7X","BMW","740i Sedan","CJ07658",0,3,4720,6140,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PBMX10075448","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0067,0.007,"0.020",0,"BMW: 740i Sedan, 740i xDrive Sedan"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.350",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.350",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.350",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.350",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.033,0.03,"0.20",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.033,0.03,"0.20",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0B5P","SBMXR0150G6F","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.02",0,"BMW: M340i Sedan, M340i xDrive Sedan, M440i Convertible, M440i Coupe, M440i Gran Coupe, M440i xDrive Convertible, M440i xDrive Coupe, M440i xDrive Gran Coupe, X3 M50i xDrive"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078641","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.27140000000000003,0.28600000000000003,"0.500",0.0151,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078641","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.27140000000000003,0.28600000000000003,"0.500",0.0151,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078642","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.27740000000000004,0.29200000000000004,"0.500",0.0151,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078642","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.27740000000000004,0.29200000000000004,"0.500",0.0151,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078643","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078643","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078644","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",1E-3,0,"0.02",0,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078644","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",1E-3,0,"0.02",0,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078645","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0,0.02,"0.20",0.02,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0170G0H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078645","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0,0.02,"0.20",0.02,"BMW: X5 xDrive50e"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078641","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.27140000000000003,0.28600000000000003,"0.500",0.0151,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078641","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.27140000000000003,0.28600000000000003,"0.500",0.0151,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078642","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.27740000000000004,0.29200000000000004,"0.500",0.0151,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078642","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.27740000000000004,0.29200000000000004,"0.500",0.0151,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078643","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078643","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078644","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",1E-3,0,"0.02",0,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078644","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",1E-3,0,"0.02",0,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078645","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0,0.02,"0.20",0.02,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ03.0H70","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078645","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0,0.02,"0.20",0.02,"BMW: 750e xDrive Sedan"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063966","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.05,"0.20",0.011000000000000001,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063966","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.043000000000000003,0.05,"0.20",0.011000000000000001,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063967","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.010700000000000001,0.011000000000000001,"0.020",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063967","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.010700000000000001,0.011000000000000001,"0.020",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064376","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1961,0.256,"0.500",0.0594,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064376","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1961,0.256,"0.500",0.0594,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064377","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.011000000000000001,0.01,"0.02",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064377","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.011000000000000001,0.01,"0.02",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064490","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.184,0.184,"0.500",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064490","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.184,0.184,"0.500",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064491","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXJ04.4S68","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064491","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: 760i xDrive Sedan, ALPINA XB7, X5 M60i xDrive, X6 M60i xDrive, X7 M60i xDrive"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075602","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1894,0.189,"0.300",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075602","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1894,0.189,"0.300",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075677","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.19090000000000001,0.191,"0.300",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075677","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.19090000000000001,0.191,"0.300",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075678","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.009000000000000001,0.01,"0.05",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075678","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.009000000000000001,0.01,"0.05",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075679","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0151,0.015000000000000001,"0.020",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075679","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0151,0.015000000000000001,"0.020",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075680","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.013000000000000001,0.01,"0.02",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075680","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.013000000000000001,0.01,"0.02",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075859","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.1,0.1,"0.20",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0B48","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075859","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.1,0.1,"0.20",0,"BMW: X1 xDrive28i, X2 xDrive28i"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075602","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1894,0.189,"0.300",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075602","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1894,0.189,"0.300",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075677","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.19090000000000001,0.191,"0.300",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075677","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.19090000000000001,0.191,"0.300",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075678","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.009000000000000001,0.01,"0.05",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075678","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.009000000000000001,0.01,"0.05",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075679","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0151,0.015000000000000001,"0.020",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075679","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0151,0.015000000000000001,"0.020",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075680","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.013000000000000001,0.01,"0.02",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075680","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.013000000000000001,0.01,"0.02",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075859","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.1,0.1,"0.20",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT02.0U1X","SBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075859","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.1,0.1,"0.20",0,"BMW: X1 M35i, X2 M35i  Mini: JCW Countryman ALL4"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.041,0.04,"0.20",1E-3,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",1E-3,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0G2X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: X4 M40i"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT03.0S58","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: X4 M, X4 M Competition"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084685","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.16790000000000002,0.183,"0.500",0.015000000000000001,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084685","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.16790000000000002,0.183,"0.500",0.015000000000000001,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084686","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1433,0.158,"0.500",0.015000000000000001,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084686","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1433,0.158,"0.500",0.015000000000000001,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084687","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084687","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084688","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.007,0.04,"0.20",0.028,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084688","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.007,0.04,"0.20",0.028,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084689","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4H09","SBMXR0170H09","BMW","XM Label","9N82497",6,4.4,6091,7209,6500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","SBMX10084689","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.02",0,"BMW: XM, XM Label"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063966","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.05,"0.20",0.011000000000000001,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063966","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.043000000000000003,0.05,"0.20",0.011000000000000001,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063967","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.010700000000000001,0.011000000000000001,"0.020",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063967","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.010700000000000001,0.011000000000000001,"0.020",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064376","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1961,0.256,"0.500",0.0594,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064376","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1961,0.256,"0.500",0.0594,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064377","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.011000000000000001,0.01,"0.02",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064377","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.011000000000000001,0.01,"0.02",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064490","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.184,0.184,"0.500",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064490","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.184,0.184,"0.500",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064491","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXT04.4S6M","SBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064491","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: X5 M Competition, X6 M Competition"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.300",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085517","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17500000000000002,0.17500000000000002,"0.300",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.300",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085519","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.300",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085522","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.033,0.03,"0.20",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085523","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.033,0.03,"0.20",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085524","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0095,0.01,"0.020",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0B4D","SBMXR0150G60","BMW","X3 xDrive30i","9T75018",0,2,4176,5512,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","SBMX10085525","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.02",0,"BMW: 530i Sedan, 530i xDrive Sedan"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.041,0.04,"0.20",1E-3,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",1E-3,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV02.0M48","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.041,0.04,"0.20",1E-3,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",1E-3,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B07","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2179,0.234,"0.300",0.0162,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.041,0.04,"0.20",1E-3,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",1E-3,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0B5X","SBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078641","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.27140000000000003,0.28600000000000003,"0.500",0.0151,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078641","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.27140000000000003,0.28600000000000003,"0.500",0.0151,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078642","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.27740000000000004,0.29200000000000004,"0.500",0.0151,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078642","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.27740000000000004,0.29200000000000004,"0.500",0.0151,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078643","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078643","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078644","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",1E-3,0,"0.02",0,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078644","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",1E-3,0,"0.02",0,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078645","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0,0.02,"0.20",0.02,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0H5P","SBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078645","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0,0.02,"0.20",0.02,"BMW: 550e xDrive Sedan"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV03.0SM3","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: M2 Coupe, M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 CS Coupe, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4N63","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: ALPINA B8 Gran Coupe, M850i xDrive Convertible, M850i xDrive Coupe, M850i xDrive Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046019","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2949,0.342,"0.450",0.047400000000000005,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046020","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046029","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.33690000000000003,0.35300000000000004,"0.450",0.0162,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046036","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.043000000000000003,0.04,"0.20",1E-3,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046037","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"BMW","SBMXV04.4SM5","SBMXR0150G3F","BMW","M550i xDrive","G463617",0,4.4,4372,5430,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JBMX10046038","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060536","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060536","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060537","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2404,0.249,"0.550",0.009000000000000001,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060537","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2404,0.249,"0.550",0.009000000000000001,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060538","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1326,0.138,"0.550",0.0057,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060538","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1326,0.138,"0.550",0.0057,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10073730","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0081,0.008,"0.020",0,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V1","SCRXF0180TP0","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10073730","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0081,0.008,"0.020",0,"RAM: ProMaster 3500 Cab Chassis"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060536","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060536","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060537","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2404,0.249,"0.550",0.009000000000000001,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060537","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2404,0.249,"0.550",0.009000000000000001,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060538","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1326,0.138,"0.550",0.0057,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060538","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1326,0.138,"0.550",0.0057,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060539","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.052000000000000005,0.05,"0.20",0,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060539","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.052000000000000005,0.05,"0.20",0,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10073730","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0081,0.008,"0.020",0,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXD03.65V2","SCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10073730","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0081,0.008,"0.020",0,"RAM: ProMaster 1500, ProMaster 2500, ProMaster 3500"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048785","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048785","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048786","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.18460000000000001,0.194,"0.300",0.009000000000000001,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048786","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.18460000000000001,0.194,"0.300",0.009000000000000001,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048788","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.065,0.06,"0.20",0,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048788","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.065,0.06,"0.20",0,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10073223","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0112,0.011000000000000001,"0.020",0,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10073223","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0112,0.011000000000000001,"0.020",0,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003599","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1384,0.14400000000000002,"0.300",0.0057,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003599","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1384,0.14400000000000002,"0.300",0.0057,"ALFA ROMEO: Giulia, Giulia AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048785","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048785","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048786","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.18460000000000001,0.194,"0.400",0.009000000000000001,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048786","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.18460000000000001,0.194,"0.400",0.009000000000000001,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048788","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.065,0.06,"0.20",0,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048788","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.065,0.06,"0.20",0,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10073248","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0085,0.008,"0.020",0,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10073248","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0085,0.008,"0.020",0,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003599","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1384,0.14400000000000002,"0.400",0.0057,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXJ02.05P2","SCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003599","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1384,0.14400000000000002,"0.400",0.0057,"ALFA ROMEO: Stelvio, Stelvio AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076922","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076922","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076923","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2048,0.21400000000000002,"0.400",0.009000000000000001,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076923","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2048,0.21400000000000002,"0.400",0.009000000000000001,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076924","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076924","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076944","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0064,0.006,"0.020",0,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076944","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0064,0.006,"0.020",0,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX91005237","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2247,0.23,"0.400",0.0057,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0110PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX91005237","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2247,0.23,"0.400",0.0057,"Jeep: Compass 4X4"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076922","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076922","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076923","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2048,0.21400000000000002,"0.400",0.009000000000000001,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076923","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2048,0.21400000000000002,"0.400",0.009000000000000001,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076924","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076924","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076944","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0064,0.006,"0.020",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076944","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0064,0.006,"0.020",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX91005237","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2247,0.23,"0.400",0.0057,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX91005237","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2247,0.23,"0.400",0.0057,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076922","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076922","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076923","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2048,0.21400000000000002,"0.400",0.009000000000000001,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076923","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2048,0.21400000000000002,"0.400",0.009000000000000001,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076924","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076924","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076944","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0064,0.006,"0.020",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076944","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0064,0.006,"0.020",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX91005237","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2247,0.23,"0.400",0.0057,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P1","SCRXR0115PP4","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX91005237","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2247,0.23,"0.400",0.0057,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05P2","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 4dr 4X4"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067516","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.16840000000000002,0.17400000000000002,"0.375",0.0057,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067516","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.16840000000000002,0.17400000000000002,"0.375",0.0057,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067517","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24400000000000002,0.253,"0.375",0.009000000000000001,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067517","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24400000000000002,0.253,"0.375",0.009000000000000001,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067518","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067518","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067519","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0155FEH","Jeep","Wrangler 4dr 4xe","L0JLX9460",0,2,5361,6400,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","MCRX10067519","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 4dr 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX10071605","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX10071605","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX10071606","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3049,0.314,"0.500",0.009000000000000001,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX10071606","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3049,0.314,"0.500",0.009000000000000001,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX10071607","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",2E-3,0,"0.20",0,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX10071607","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",2E-3,0,"0.20",0,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX91004881","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2545,0.26,"0.500",0.0057,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT02.05PH","SCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX91004881","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2545,0.26,"0.500",0.0057,"Jeep: Grand Cherokee 4xe"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Jeep: Grand Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 HO 4x4, 1500 HO 4x4 (20 inch wheels)"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075664","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.334,0.34,"0.550",0.0057,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075664","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.334,0.34,"0.550",0.0057,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075665","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075665","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075666","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4813,0.49,"0.550",0.009000000000000001,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075666","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4813,0.49,"0.550",0.009000000000000001,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075667","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.041,0.04,"0.20",0,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075667","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",0,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075695","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0146,0.015000000000000001,"0.020",0,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P2","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075695","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0146,0.015000000000000001,"0.020",0,"Jeep: Grand Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P3","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 RHO 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049480","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.40650000000000003,0.41200000000000003,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049480","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.40650000000000003,0.41200000000000003,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049481","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3013,0.31,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049481","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3013,0.31,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049482","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049482","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049483","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.03,0.03,"0.20",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049483","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.03,0.03,"0.20",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074520","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",5.8000000000000005E-3,0.006,"0.020",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074520","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",5.8000000000000005E-3,0.006,"0.020",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075664","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.334,0.34,"0.550",0.0057,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075664","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.334,0.34,"0.550",0.0057,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075665","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075665","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075666","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4813,0.49,"0.550",0.009000000000000001,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075666","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4813,0.49,"0.550",0.009000000000000001,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075667","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.041,0.04,"0.20",0,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075667","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",0,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075695","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0146,0.015000000000000001,"0.020",0,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.05P4","SCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075695","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0146,0.015000000000000001,"0.020",0,"Jeep: Wagoneer L 4x2, Wagoneer L 4x4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 2dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044755","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.045000000000000005,0.04,"0.20",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044755","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.045000000000000005,0.04,"0.20",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044760","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34700000000000003,0.35300000000000004,"0.450",0.0057,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044760","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.34700000000000003,0.35300000000000004,"0.450",0.0057,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044761","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3431,0.35200000000000004,"0.450",0.009000000000000001,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044761","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3431,0.35200000000000004,"0.450",0.009000000000000001,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044762","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044762","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10076772","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0074,0.007,"0.020",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10076772","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0074,0.007,"0.020",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Gladiator 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Wrangler 4dr 4X4, Wrangler Rubicon 4dr 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P5","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango Pursuit AWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4, Grand Cherokee L 4X2, Grand Cherokee L 4X4"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044755","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.045000000000000005,0.04,"0.20",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044755","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.045000000000000005,0.04,"0.20",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044760","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34700000000000003,0.35300000000000004,"0.450",0.0057,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044760","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.34700000000000003,0.35300000000000004,"0.450",0.0057,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044761","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3431,0.35200000000000004,"0.450",0.009000000000000001,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044761","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3431,0.35200000000000004,"0.450",0.009000000000000001,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044762","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044762","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10076772","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0074,0.007,"0.020",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10076772","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0074,0.007,"0.020",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65P6","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045053","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.053000000000000005,0.05,"0.20",0,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045053","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.053000000000000005,0.05,"0.20",0,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045054","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1829,0.192,"0.450",0.009000000000000001,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045054","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1829,0.192,"0.450",0.009000000000000001,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045055","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045055","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045056","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24180000000000001,0.248,"0.450",0.0057,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PH","SCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045056","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24180000000000001,0.248,"0.450",0.0057,"Chrysler: Pacifica Hybrid"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049480","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.40650000000000003,0.41200000000000003,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049480","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.40650000000000003,0.41200000000000003,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049481","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3013,0.31,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049481","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3013,0.31,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049482","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049482","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049483","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.03,0.03,"0.20",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049483","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.03,0.03,"0.20",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074520","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",5.8000000000000005E-3,0.006,"0.020",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074520","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",5.8000000000000005E-3,0.006,"0.020",0,"RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074521","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.65PN","SCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 4X2, 1500 4X4"]
[2025,"FCA US LLC","SCRXT03.6FP7","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango Pursuit AWD"]
[2025,"FCA US LLC","SCRXT03.6FP7","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango Pursuit AWD"]
[2025,"FCA US LLC","SCRXT03.6FP7","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango Pursuit AWD"]
[2025,"FCA US LLC","SCRXT03.6FP7","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango Pursuit AWD"]
[2025,"FCA US LLC","SCRXT03.6FP7","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango Pursuit AWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT05.75P0","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXT06.25P1","SCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango SRT AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Alfa Romeo","Tonale eAWD","L2ALF8457",0,1.3,4158,5335,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"Y","RCRX10078876","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2369,0.24600000000000002,"0.300",0.009000000000000001,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Alfa Romeo","Tonale eAWD","L2ALF8457",0,1.3,4158,5335,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"Y","RCRX10078876","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2369,0.24600000000000002,"0.300",0.009000000000000001,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Alfa Romeo","Tonale eAWD","L2ALF8457",0,1.3,4158,5335,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"Y","RCRX10078877","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1864,0.192,"0.300",0.0057,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Alfa Romeo","Tonale eAWD","L2ALF8457",0,1.3,4158,5335,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"Y","RCRX10078877","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1864,0.192,"0.300",0.0057,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Alfa Romeo","Tonale eAWD","L2ALF8457",0,1.3,4158,5335,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"Y","RCRX10078879","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.075,0.08,"0.20",0,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Alfa Romeo","Tonale eAWD","L2ALF8457",0,1.3,4158,5335,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"Y","RCRX10078879","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.075,0.08,"0.20",0,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045055","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"FCA US LLC","SCRXV01.35PH","SCRXR0082FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045055","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"ALFA ROMEO: Tonale eAWD  Dodge: Hornet PHEV AWD"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",0,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073814","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","120","LEAK-DIA",0,0,"0.02",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",0,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073814","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","120","LEAK-DIA",0,0,"0.02",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073820","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1825,0.182,"0.275",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073820","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.1825,0.182,"0.275",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073821","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.064,0.06,"0.20",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073821","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","120","HC",0.064,0.06,"0.20",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073822","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2146,0.215,"0.275",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073822","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.2146,0.215,"0.275",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073959","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.026000000000000002,0.03,"0.05",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV02.9HYB","SFEXR017506H","Ferrari","296 GTB Spider","257806",1,2.9,3902,4542,4250,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","PFEX10073959","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.026000000000000002,0.03,"0.05",0,"Ferrari North America, Inc.: 296 GTB, 296 GTS"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080361","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.15,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080361","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.15,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080363","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.19,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080363","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.19,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080365","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.11960000000000001,0.12,"0.200",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080366","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2.1000000000000003E-3,2E-3,"0.050",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080366","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",2.1000000000000003E-3,2E-3,"0.050",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080367","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","120","LEAK-DIA",0.0002,0,"0.002",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9H70","SFEXR017508S","Ferrari","F173 HGC","280505",0,3.9,4101,4641,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","RFEX10080367","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","LEAK-DIA",0.0002,0,"0.002",0,"Ferrari North America, Inc.: SF90 XX Spider, SF90 XX Stradale"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10067547","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.02,0.02,"0.200",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10067549","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.004,0.004,"0.050",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10067549","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.004,0.004,"0.050",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10067717","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","120","LEAK-DIA",3.0000000000000003E-4,0,"0.002",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10067717","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","LEAK-DIA",3.0000000000000003E-4,0,"0.002",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10073453","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.19,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10073453","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.19,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10079868","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.19,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9HYB","SFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10079868","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.19,0.2,"0.3",0,"Ferrari North America, Inc.: SF90 Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",0,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079849","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",0,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079849","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.02",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079137","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.10360000000000001,0.10400000000000001,"0.275",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079137","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.10360000000000001,0.10400000000000001,"0.275",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079140","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1267,0.127,"0.275",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079140","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1267,0.127,"0.275",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079146","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0061,0.006,"0.050",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079146","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0061,0.006,"0.050",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079149","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079149","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.02",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079151","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.004,0,"0.20",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV03.9T50","SFEXR017508K","Ferrari","F164 BCC","272661",1,3.9,3814,4729,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","RFEX10079151","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.004,0,"0.20",0,"Ferrari North America, Inc.: Roma Spider"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073328","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",3.0000000000000003E-4,0,"0.020",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073328","MFR","67","Leak Test - Port Near Canister","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",3.0000000000000003E-4,0,"0.020",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073347","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0074,0.007,"0.020",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073347","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0074,0.007,"0.020",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073363","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22010000000000002,0.22,"0.325",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073363","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22010000000000002,0.22,"0.325",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073408","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2717,0.272,"0.325",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073408","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2717,0.272,"0.325",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073410","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.166,0.17,"0.20",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073410","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.166,0.17,"0.20",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073414","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0108,0.011000000000000001,"0.050",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"Ferrari","SFEXV06.5GDI","SFEXR017512D","Ferrari","Ferrari Daytona SP3","266323",0,6.5,3627,4123,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","PFEX10073414","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0108,0.011000000000000001,"0.050",0,"Ferrari North America, Inc.: Ferrari Daytona SP3"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",3.8E-3,0.004,"0.020",0,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",3.8E-3,0.004,"0.020",0,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Ford","Escape","LTC1-1.5-H-527",0,1.5,3514,4760,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058645","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Ford","Escape","LTC1-1.5-H-527",0,1.5,3514,4760,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058645","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Ford","Escape","LTC1-1.5-H-527",0,1.5,3514,4760,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058646","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.1913,0.191,"0.300",0,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Ford","Escape","LTC1-1.5-H-527",0,1.5,3514,4760,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058646","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1913,0.191,"0.300",0,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Lincoln","Corsair","LTF1-2.0-H-543",0,2,3997,4940,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058648","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.056,0.06,"0.20",2E-3,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDE","Lincoln","Corsair","LTF1-2.0-H-543",0,2,3997,4940,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058648","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.056,0.06,"0.20",2E-3,"Ford: ESCAPE FWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087231","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2929,0.29300000000000004,"0.400",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087231","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2929,0.29300000000000004,"0.400",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087244","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.3523,0.35200000000000004,"0.400",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087244","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3523,0.35200000000000004,"0.400",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087245","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087245","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087246","MFR","24","Federal fuel refueling test (ORVR)","58","Tier 3 E10 Regular Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.016,0.02,"0.20",2E-3,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087246","MFR","24","Federal fuel refueling test (ORVR)","58","Tier 3 E10 Regular Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.016,0.02,"0.20",2E-3,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",3.8E-3,0.004,"0.020",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT01.52X1","SFMXR0125GDF","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",3.8E-3,0.004,"0.020",0,"Ford: ESCAPE AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087231","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2929,0.29300000000000004,"0.400",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087231","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2929,0.29300000000000004,"0.400",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087244","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.3523,0.35200000000000004,"0.400",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087244","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3523,0.35200000000000004,"0.400",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087245","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",2E-3,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087245","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",2E-3,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087246","MFR","24","Federal fuel refueling test (ORVR)","58","Tier 3 E10 Regular Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.016,0.02,"0.20",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","BRONCO SPORT SASQUATCH","SHD1-1.5-J-989",1,1.5,3733,4810,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","SFMX10087246","MFR","24","Federal fuel refueling test (ORVR)","58","Tier 3 E10 Regular Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.016,0.02,"0.20",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",3.8E-3,0.004,"0.020",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0125GDF","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",3.8E-3,0.004,"0.020",0,"Ford: ESCAPE AWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","318W879",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079536","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.004,0.004,"0.020",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","318W879",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079536","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.004,0.004,"0.020",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079453","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2031,0.203,"0.400",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079453","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2031,0.203,"0.400",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079533","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.19090000000000001,0.191,"0.400",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079533","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.19090000000000001,0.191,"0.400",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079534","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079534","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079535","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.017,0.02,"0.20",1E-3,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JB","SFMXR0140NDN","Ford","RANGER RAPTOR 4WD","RRD1-3.0-J-731",0,3,5379,6790,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10079535","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.017,0.02,"0.20",1E-3,"Lincoln: NAUTILUS AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082346","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2134,0.22,"0.400",6.3E-3,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082346","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2134,0.22,"0.400",6.3E-3,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082347","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.15960000000000002,0.166,"0.400",6.3E-3,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082347","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.15960000000000002,0.166,"0.400",6.3E-3,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082348","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082348","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082349","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.005,0,"0.20",0,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.02JF","SFMXR0180LDF","Ford","NAUTILUS HEV AWD","RD91-2.0-J-877",0,2,4667,5787,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","RFMX10082349","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.005,0,"0.20",0,"Lincoln: NAUTILUS HEV AWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.17300000000000001,0.17300000000000001,"0.400",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17300000000000001,0.17300000000000001,"0.400",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.171,0.171,"0.400",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.171,0.171,"0.400",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"000.05",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"000.05",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",0,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060474","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",3.3E-3,0.003,"0.020",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",0,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060474","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.3E-3,0.003,"0.020",0,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.008,0.01,"0.20",1E-3,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.34K2","SFMXR0185NDF","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"000.20",1E-3,"Ford: EXPLORER AWD, EXPLORER RWD"]
[2025,"FOMOCO","SFMXT02.52F1","SFMXR0135LDF","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10060716","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",0,"Ford: ESCAPE AWD HEV, ESCAPE FWD HEV"]
[2025,"FOMOCO","SFMXT02.52F1","SFMXR0135LDF","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10060716","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",0,"Ford: ESCAPE AWD HEV, ESCAPE FWD HEV"]
[2025,"FOMOCO","SFMXT02.52F1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Ford: ESCAPE AWD HEV, ESCAPE FWD HEV"]
[2025,"FOMOCO","SFMXT02.52F1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Ford: ESCAPE AWD HEV, ESCAPE FWD HEV"]
[2025,"FOMOCO","SFMXT02.52F1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063695","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: ESCAPE AWD HEV, ESCAPE FWD HEV"]
[2025,"FOMOCO","SFMXT02.52F1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063695","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: ESCAPE AWD HEV, ESCAPE FWD HEV"]
[2025,"FOMOCO","SFMXT02.52P1","SFMXR0135LDF","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10060716","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.006,0.01,"0.20",0,"Ford: ESCAPE FWD PHEV"]
[2025,"FOMOCO","SFMXT02.52P1","SFMXR0135LDF","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10060716","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",0,"Ford: ESCAPE FWD PHEV"]
[2025,"FOMOCO","SFMXT02.52P1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Ford: ESCAPE FWD PHEV"]
[2025,"FOMOCO","SFMXT02.52P1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Ford: ESCAPE FWD PHEV"]
[2025,"FOMOCO","SFMXT02.52P1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063695","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: ESCAPE FWD PHEV"]
[2025,"FOMOCO","SFMXT02.52P1","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063695","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: ESCAPE FWD PHEV"]
[2025,"FOMOCO","SFMXT02.53CE","SFMXR0135LDF","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10060716","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.006,0.01,"0.20",0,"Lincoln: CORSAIR AWD PHEV"]
[2025,"FOMOCO","SFMXT02.53CE","SFMXR0135LDF","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10060716","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",0,"Lincoln: CORSAIR AWD PHEV"]
[2025,"FOMOCO","SFMXT02.53CE","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Lincoln: CORSAIR AWD PHEV"]
[2025,"FOMOCO","SFMXT02.53CE","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Lincoln: CORSAIR AWD PHEV"]
[2025,"FOMOCO","SFMXT02.53CE","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063695","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Lincoln: CORSAIR AWD PHEV"]
[2025,"FOMOCO","SFMXT02.53CE","SFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063695","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Lincoln: CORSAIR AWD PHEV"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.17300000000000001,0.17300000000000001,"0.500",0,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17300000000000001,0.17300000000000001,"0.500",0,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.171,0.171,"0.500",0,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.171,0.171,"0.500",0,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.008,0.01,"0.20",1E-3,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.03U2","SFMXR0185NDG","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.20",1E-3,"Ford: EXPLORER AWD, EXPLORER RWD, INTERCEPTOR UTILITY AWD  Lincoln: AVIATOR AWD, AVIATOR RWD"]
[2025,"FOMOCO","SFMXT03.33F1","SFMXR0165LDG","Ford","Explorer Police FHEV","LTW1-3.3-L-471",0,3.3000000000000003,5095,6840,5500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","LFMX10059621","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",2E-3,0,"0.20",2E-3,"Ford: INTERCEPTOR UTILITY HEV AWD"]
[2025,"FOMOCO","SFMXT03.33F1","SFMXR0165LDG","Ford","Explorer Police FHEV","LTW1-3.3-L-471",0,3.3000000000000003,5095,6840,5500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","LFMX10059621","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.20",2E-3,"Ford: INTERCEPTOR UTILITY HEV AWD"]
[2025,"FOMOCO","SFMXT03.33F1","SFMXR0165LDG","Ford","Explorer Police FHEV","LTW1-3.3-L-471",0,3.3000000000000003,5095,6840,5500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","LFMX10059622","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",2E-3,"Ford: INTERCEPTOR UTILITY HEV AWD"]
[2025,"FOMOCO","SFMXT03.33F1","SFMXR0165LDG","Ford","Explorer Police FHEV","LTW1-3.3-L-471",0,3.3000000000000003,5095,6840,5500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","LFMX10059622","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"000.05",2E-3,"Ford: INTERCEPTOR UTILITY HEV AWD"]
[2025,"FOMOCO","SFMXT03.33F1","SFMXR0165LDG","Ford","Explorer Police FHEV","LTW1-3.3-L-471",0,3.3000000000000003,5095,6840,5500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","LFMX10059623","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.21380000000000002,0.21400000000000002,"0.500",0,"Ford: INTERCEPTOR UTILITY HEV AWD"]
[2025,"FOMOCO","SFMXT03.33F1","SFMXR0165LDG","Ford","Explorer Police FHEV","LTW1-3.3-L-471",0,3.3000000000000003,5095,6840,5500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","LFMX10059623","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.21380000000000002,0.21400000000000002,"0.500",0,"Ford: INTERCEPTOR UTILITY HEV AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.17300000000000001,0.17300000000000001,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.17300000000000001,0.17300000000000001,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17300000000000001,0.17300000000000001,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083318","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17300000000000001,0.17300000000000001,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.171,0.171,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.171,0.171,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.171,0.171,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083319","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.171,0.171,"0.500",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","Explorer AWD","RTW1-2.3-J-780",0,2.3000000000000003,4596,5940,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","SFMX10083320","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",null,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",0,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060474","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",3.3E-3,0.003,"0.020",0,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",0,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060474","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",3.3E-3,0.003,"0.020",0,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",0,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060474","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.3E-3,0.003,"0.020",0,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",0,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060474","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.3E-3,0.003,"0.020",0,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.008,0.01,"0.20",1E-3,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT03.33U3","SFMXR0185NDG","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.20",1E-3,"Ford: INTERCEPTOR UTILITY AWD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F-150","JFC1-2.7-032",0,2.7,4903,7000,5250,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047781","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2989,0.299,"0.500",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F-150","JFC1-2.7-032",0,2.7,4903,7000,5250,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047781","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2989,0.299,"0.500",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F-150","JFC1-2.7-032",0,2.7,4903,7000,5250,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047782","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F-150","JFC1-2.7-032",0,2.7,4903,7000,5250,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047782","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F-150","JFC1-2.7-032",0,2.7,4903,7000,5250,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10048127","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.01,0.01,"0.020",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F-150","JFC1-2.7-032",0,2.7,4903,7000,5250,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10048127","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.01,0.01,"0.020",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F150-Super Cab gas 4x4","JFC1-3.3-033",2,3.3000000000000003,4687,6500,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JFMX10049684","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.016,0.03,"0.20",0.013000000000000001,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0200GDG","Ford","F150-Super Cab gas 4x4","JFC1-3.3-033",2,3.3000000000000003,4687,6500,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JFMX10049684","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.016,0.03,"0.20",0.013000000000000001,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049672","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.1981,0.198,"0.500",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049672","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1981,0.198,"0.500",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049673","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2212,0.221,"0.500",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049673","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2212,0.221,"0.500",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049674","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",1E-3,0,"0.05",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049674","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",2,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049676","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.008,0.01,"0.20",0.003,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",2,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049676","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.20",0.003,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",2,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049769","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.010700000000000001,0.011000000000000001,"0.020",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"FOMOCO","SFMXT05.03DP","SFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",2,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049769","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.010700000000000001,0.011000000000000001,"0.020",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 PICKUP TREMOR 4WD"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064690","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.38620000000000004,0.386,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064690","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.38620000000000004,0.386,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064691","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064691","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","SILVERADO 2WD","66CRLN1016",0,6.6000000000000005,6761,10350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057630","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0183,0.018000000000000002,"0.030",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXF02176BB","CHEVROLET","SILVERADO 2WD","66CRLN1016",0,6.6000000000000005,6761,10350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057630","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0183,0.018000000000000002,"0.030",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064545","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.39990000000000003,0.4,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064545","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.39990000000000003,0.4,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064546","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.053000000000000005,0.05,"0.20",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064546","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.053000000000000005,0.05,"0.20",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064547","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064547","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064548","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.5321,0.532,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064548","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.5321,0.532,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064746","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0108,0.011000000000000001,"0.030",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD04.3170","SGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064746","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0108,0.011000000000000001,"0.030",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075100","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",3.6000000000000003E-3,0.004,"0.030",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075100","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.6000000000000003E-3,0.004,"0.030",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075101","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","SPITBACK",0.05,0,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075101","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.05,0,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075103","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3039,0.304,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075103","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3039,0.304,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075104","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075104","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075105","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4481,0.448,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075105","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4481,0.448,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064690","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.38620000000000004,0.386,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064690","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.38620000000000004,0.386,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064691","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064691","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","SILVERADO 2WD","66CRLN1016",0,6.6000000000000005,6761,10350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057630","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0183,0.018000000000000002,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXF02176BB","CHEVROLET","SILVERADO 2WD","66CRLN1016",0,6.6000000000000005,6761,10350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057630","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0183,0.018000000000000002,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080778","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3629,0.36300000000000004,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080778","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3629,0.36300000000000004,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080779","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",4.3E-3,0.004,"0.030",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080779","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",4.3E-3,0.004,"0.030",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080780","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.5096,0.51,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080780","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.5096,0.51,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080781","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.036000000000000004,0.04,"0.20",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080781","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.036000000000000004,0.04,"0.20",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080782","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR017160E","CHEVROLET","G3500 EXPRESS 2WD PASS","66R10003EX",0,6.6000000000000005,6664,9900,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RGMX10080782","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078340","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.014,0.01,"0.20",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078340","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.014,0.01,"0.20",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078341","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078341","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078342","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34840000000000004,0.34800000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078342","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.34840000000000004,0.34800000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078343","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.005200000000000001,0.005,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078343","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.005200000000000001,0.005,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX91005307","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.28650000000000003,0.28600000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6170","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX91005307","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.28650000000000003,0.28600000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057419","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3247,0.325,"0.600",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057419","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3247,0.325,"0.600",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057420","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057420","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057421","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.44830000000000003,0.448,"0.600",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057421","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.44830000000000003,0.448,"0.600",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057423","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","SPITBACK",0.11,0.1,"1.0",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057423","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.11,0.1,"1.0",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10064431","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.019200000000000002,0.019,"0.030",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CDLN1053",0,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10064431","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.019200000000000002,0.019,"0.030",0,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075100","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",3.6000000000000003E-3,0.004,"0.030",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075100","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.6000000000000003E-3,0.004,"0.030",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075101","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","SPITBACK",0.05,0,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075101","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.05,0,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075103","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3039,0.304,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075103","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3039,0.304,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075104","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075104","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075105","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4481,0.448,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075105","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4481,0.448,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064690","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.38620000000000004,0.386,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064690","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.38620000000000004,0.386,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064691","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064691","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","SILVERADO 2WD","66CRLN1016",0,6.6000000000000005,6761,10350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057630","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0183,0.018000000000000002,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXF02176BB","CHEVROLET","SILVERADO 2WD","66CRLN1016",0,6.6000000000000005,6761,10350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057630","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0183,0.018000000000000002,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078340","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.014,0.01,"0.20",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078340","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.014,0.01,"0.20",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078341","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078341","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078342","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34840000000000004,0.34800000000000003,"0.600",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078342","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.34840000000000004,0.34800000000000003,"0.600",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078343","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.005200000000000001,0.005,"0.030",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078343","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.005200000000000001,0.005,"0.030",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX91005307","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.28650000000000003,0.28600000000000003,"0.600",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6230","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX91005307","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.28650000000000003,0.28600000000000003,"0.600",0,"Chevrolet: SILERAVDO 3500 HD 4WD MT, SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 2500 HD 4WD ZR2, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD AT4X, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW, SIERRA 3500 HD 4WD MT"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078340","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.014,0.01,"0.20",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078340","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.014,0.01,"0.20",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078341","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078341","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078342","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34840000000000004,0.34800000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078342","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.34840000000000004,0.34800000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078343","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.005200000000000001,0.005,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX10078343","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.005200000000000001,0.005,"0.030",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX91005307","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.28650000000000003,0.28600000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXD06.6378","SGMXR021360B","GMC","SIERRA 2500 HD 2WD","66CRRV1140",0,6.6000000000000005,6800,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","RGMX91005307","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.28650000000000003,0.28600000000000003,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 2500 HD 4WD MT, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 2WD DRW, SILVERADO 3500 HD 4WD, SILVERADO 3500 HD 4WD DRW  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 2500 HD 4WD MT, SIERRA 3500 HD 2WD, SIERRA 3500 HD 2WD DRW, SIERRA 3500 HD 4WD, SIERRA 3500 HD 4WD DRW"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084487","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.277,0.277,"0.350",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084487","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.277,0.277,"0.350",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084488","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.038,0.04,"0.20",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084488","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.038,0.04,"0.20",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084489","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084489","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084490","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22290000000000001,0.223,"0.350",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084490","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22290000000000001,0.223,"0.350",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084491","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",3.1000000000000003E-3,0.003,"0.020",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT01.5080","SGMXR010235A","CHEVROLET","EQUINOX FWD","151SXV5644",0,1.5,3468,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","SGMX10084491","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.1000000000000003E-3,0.003,"0.020",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035626","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2316,0.232,"0.400",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035626","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2316,0.232,"0.400",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035627","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2189,0.219,"0.400",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035627","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2189,0.219,"0.400",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035628","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035628","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035629","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.026000000000000002,0.03,"0.20",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035629","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.026000000000000002,0.03,"0.20",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10053626","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.004,0.004,"0.020",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0400","SGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10053626","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.004,0.004,"0.020",0,"Buick: ENVISION AWD  Cadillac: XT4 AWD, XT4 FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061439","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.024,0.02,"0.20",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061439","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.024,0.02,"0.20",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061440","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.29150000000000004,0.29200000000000004,"0.450",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061440","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.29150000000000004,0.29200000000000004,"0.450",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061441","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061441","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061442","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.012100000000000001,0.012,"0.020",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061442","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.012100000000000001,0.012,"0.020",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX91004483","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2636,0.264,"0.450",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0500","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX91004483","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2636,0.264,"0.450",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061439","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.024,0.02,"0.20",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061439","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.024,0.02,"0.20",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061440","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.29150000000000004,0.29200000000000004,"0.450",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061440","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.29150000000000004,0.29200000000000004,"0.450",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061441","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061441","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061442","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.012100000000000001,0.012,"0.020",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061442","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.012100000000000001,0.012,"0.020",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX91004483","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2636,0.264,"0.450",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.0550","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX91004483","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2636,0.264,"0.450",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061439","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.024,0.02,"0.20",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061439","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.024,0.02,"0.20",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061440","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.29150000000000004,0.29200000000000004,"0.450",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061440","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.29150000000000004,0.29200000000000004,"0.450",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061441","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061441","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061442","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.012100000000000001,0.012,"0.020",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061442","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.012100000000000001,0.012,"0.020",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX91004483","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2636,0.264,"0.450",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT02.5000","SGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX91004483","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2636,0.264,"0.450",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Chevrolet: TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040173","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.33390000000000003,0.334,"0.425",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040173","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.33390000000000003,0.334,"0.425",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040174","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.343,0.343,"0.425",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040174","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.343,0.343,"0.425",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040175","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040175","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040176","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.051000000000000004,0.05,"0.20",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040176","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.051000000000000004,0.05,"0.20",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10051682","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.009000000000000001,0.009000000000000001,"0.020",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT03.6151","SGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10051682","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.009000000000000001,0.009000000000000001,"0.020",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053898","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1998,0.2,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053898","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1998,0.2,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053899","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1981,0.198,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053899","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1981,0.198,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053900","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053900","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10054575","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0083,0.008,"0.020",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10054575","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0083,0.008,"0.020",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27KPKN1422",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053403","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.02,0.02,"0.20",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR017350D","GMC","K10 SIERRA 4WD","27KPKN1422",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053403","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.02,0.02,"0.20",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD MUD TERRAIN TIRES, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055636","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4646,0.465,"0.525",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055636","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4646,0.465,"0.525",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055637","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.20",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055637","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.018000000000000002,0.02,"0.20",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055638","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.314,0.314,"0.525",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055638","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.314,0.314,"0.525",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055639","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055639","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055693","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.012,0.012,"0.020",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3330","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055693","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.012,0.012,"0.020",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053898","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1998,0.2,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053898","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1998,0.2,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053899","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1981,0.198,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053899","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1981,0.198,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053900","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053900","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10054575","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0083,0.008,"0.020",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT05.3387","SGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10054575","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0083,0.008,"0.020",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2025,"GM","SGMXT06.2375","SGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055693","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.012,0.012,"0.020",0,"Cadillac: ESCALADE 2WD, ESCALADE 4WD  Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2025,"GM","SGMXV03.6043","SGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10060941","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2514,0.251,"0.300",0,"Cadillac: CT4 V, CT5, CT5 AWD, CT5 V, CT5 V AWD"]
[2025,"GM","SGMXV06.2094","SGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10060942","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Cadillac: CT5 V"]
[2025,"Honda","SHNXT03.0HTC","SHNXR0150CBA","ACURA","RDX AWD A-SPEC","EKYF4A",0,2,4087,5027,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KHNX10052114","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Acura: MDX AWD Type-S"]
[2025,"Honda","SHNXV01.54EC","SHNXR0122ABA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044298","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0044,0.004,"0.020",0,"Acura: INTEGRA, INTEGRA A-SPEC"]
[2025,"Honda","SHNXV02.02EC","SHNXR0122AAA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044204","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.20",0,"Honda: HR-V AWD, HR-V FWD"]
[2025,"Honda","SHNXV02.0GES","SHNXR0112DAA","HONDA","CIVIC 4Dr","ESMC2C",7,2,3252,4146,3500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y","SHNX10084667","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.21050000000000002,0.24,"0.300",0.03,"Honda: CIVIC 4Dr, CIVIC 5Dr"]
[2025,"Hyundai","SHYXT01.6L13","SHYXR0135L1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064842","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0077,0.008,"0.020",0,"HYUNDAI MOTOR COMPANY: Tucson Hybrid, Tucson Hybrid Blue"]
[2025,"Hyundai","SHYXT02.5LR3","SHYXR0125LRG","HYUNDAI","Tucson","NX4U1H5GA095A",0,2.5,3647,4861,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NHYX10066722","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.267,0.267,"0.300",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2025,"Hyundai","SHYXT02.5VR3","SHYXR0145VRG","Kia","Sorento","MQ4U1H5GA042A",0,2.5,3935,5467,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10065286","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.020",0,"HYUNDAI MOTOR COMPANY: Santa Cruz AWD, Santa Cruz FWD"]
[2025,"Hyundai","SHYXV01.6C13","SHYXR0119C1G","KIA","NIRO","DE-U1G6GD423F",0,1.6,3274,4255,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10065784","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1723,0.17200000000000001,"0.300",0,"HYUNDAI MOTOR COMPANY: Elantra Hybrid, Elantra Hybrid Blue"]
[2025,"Hyundai","SHYXV01.6M13","SHYXR0137M1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064840","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24180000000000001,0.24200000000000002,"0.300",0,"HYUNDAI MOTOR COMPANY: Santa Fe Hybrid AWD, Santa Fe Hybrid FWD"]
[2025,"Hyundai","SHYXV02.5ER3","SHYXR0131ERG","Hyundai","Sonata","DN8U0H5GA023F",0,2.5,3120,4354,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LHYX10059891","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"HYUNDAI MOTOR COMPANY: Sonata AWD, Sonata FWD"]
[2025,"Hyundai","SHYXV02.5UP7","SHYXR0142UPG","Genesis","G80","RG3U1L5TA082A",0,3.5,4497,5567,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX10062681","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"GENESIS: GV70 AWD, GV70 RWD"]
[2025,"Hyundai","SHYXV03.5UT7","SHYXR0142UTG","Genesis","G80","RG3U1L5TA082A",0,3.5,4497,5567,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX91004651","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.20720000000000002,0.20700000000000002,"0.300",0,"GENESIS: GV70 AWD"]
[2025,"Jaguar Land Rover L","SJLXJ03.0FSC","SJLXR0140P1Z","Jaguar","F-PACE","4AMTTS512",1,5,4740,5705,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","SJLX10082903","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.02,0.02,"0.20",0,"Jaguar: F-PACE MHEV  Land Rover: Range Rover Velar P340 MHEV, Range Rover Velar P400 MHEV"]
[2025,"Jaguar Land Rover L","SJLXT02.0RTW","SJLXR0175P1Z","Land Rover","Range Rover","LKFVP004",0,3,5334,6724,5500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FJLX10033667","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.216,0.24400000000000002,"0.500",0.028,"Land Rover: Discovery"]
[2025,"Jaguar Land Rover L","SJLXT03.0HTV","SJLXR0175P1B","LAND ROVER","New Range Rover","3KMVP032",0,4.4,5705,7385,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NJLX10073373","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0109,0.011000000000000001,"0.020",0,"Land Rover: Range Rover P360 LWB MHEV, Range Rover P360 MHEV, Range Rover P400 LWB MHEV, Range Rover P400 MHEV, Range Rover Sport P360 MHEV, Range Rover Sport P400 MHEV"]
[2025,"Jaguar Land Rover L","SJLXT04.4GTH","SJLXR0175P1B","LAND ROVER","New Range Rover","3KMVP032",0,4.4,5705,7385,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NJLX10072655","MFR","24","Federal fuel refueling test (ORVR)","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.07300000000000001,0.07,"0.20",0,"Land Rover: Defender 110 MHEV"]
[2025,"Kia","SKMXT01.6P2T","SKMXR0106P2G","KIA","Sorento PHEV","MQ4U2G6TA565A",0,1.6,4537,5952,4750,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","NKMX10068151","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.020",0,"KIA: Sportage Plug-in Hybrid"]
[2025,"Kia","SKMXT02.5JR3","SKMXR0144JRG","Kia","Sorento","MQ4U1H5GA042A",0,2.5,3935,5467,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10065284","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2346,0.23500000000000001,"0.400",0,"KIA: Sorento AWD, Sorento FWD"]
[2025,"Kia","SKMXT03.5KU5","SKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA069F",0,3.5,4535,6041,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NKMX10066870","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0061,0.006,"0.020",0,"KIA: Carnival"]
[2025,"Kia","SKMXV02.0BE3","SKMXR0114BEG","HYUNDAI","VELOSTER","JS9N0GU01AC",0,2,2844,3748,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","KHYX10051004","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.033,0.04,"0.20",0.003,"KIA: Soul, Soul Eco dynamics"]
[2025,"Maserati","SMAXJ03.0TJI","SMAXR0150189","Maserati","Granturismo Trofeo","380671",0,3,4072,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RMAX10076952","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1627,0.168,"0.300",0.0057,"MASERATI: Grancabrio Modena, Grancabrio Trofeo, Granturismo Modena, Granturismo Trofeo"]
[2025,"MAZDA","STKXT02.5CDE","STKXR0117GCQ","MAZDA","CX-5","7EFPYS1-032",0,2.5,3527,4515,3875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HTKX10045490","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.014100000000000001,0.014,"0.020",0,"MAZDA: CX-5 4WD"]
[2025,"MAZDA","STKXT03.3DHB","STKXR0132GDQ","MAZDA","MAZDA CX-90","4DBH3TG1-013",0,3.3000000000000003,4903,6854,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"N","N",null,null,"Y","RTKX10077843","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","B","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2146,0.215,"0.500",0,"MAZDA: MAZDA CX-70 4WD, MAZDA CX-90 4WD"]
[2025,"Mercedes-Benz","SMBXJ02.0HY3","SMBXR0095LNA","Mercedes-Benz","AMG GLB 35 4MATIC","X247E20DETC-Z2128",2,1.991,4114,5430,4500,"F","2-Wheel Drive, Front","AM","Automated Manual",null,8,"Y","N",null,null,"N","NMBX91004809","EPA","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.29450000000000004,0.29400000000000004,"0.300",0,"Mercedes-Benz: CLA 250, CLA 250 4MATIC, GLA 250, GLA 250 4MATIC, GLB 250, GLB 250 4MATIC"]
[2025,"Mercedes-Benz","SMBXT03.0HY1","SMBXR0170LNC","Mercedes-Benz","GLS 580 4MATIC","X167E40DETC-Z2030",4,3.982,5828,7480,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"Y","MMBX10066454","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Mercedes-Benz: G 550"]
[2025,"Mercedes-Benz","SMBXV02.0HY1","SMBXR0140LNC","Mercedes-Benz","C 300 4MATIC","W206E20DETC-Z2306",1,1.999,4019,5148,4250,"A","All Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","PMBX10076307","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","OMHCE",0.014,0.03,"0.20",0.016,"Mercedes-Benz: C 300, C 300 4MATIC, CLE 300 4MATIC (Coupe), CLE 300 4MATIC (convertible), E 350, E 350 4MATIC"]
[2025,"Mercedes-Benz","SMBXV03.0HY3","SMBXR0170LNS","Mercedes-Benz","S 580 4MATIC","V223E40DETC-Z2148",0,3.982,4942,6210,5250,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","MMBX10068172","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","OMHCE",1E-3,0.02,"0.20",0.016,"Mercedes-Benz: S 500 4MATIC"]
[2025,"Mercedes-Benz","SMBXV04.0HY5","SMBXR0160LNP","Mercedes-Benz","S 580e 4MATIC","V223E30DETC-Z2304",0,2.999,5813,6768,6000,"A","All Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","PMBX10078679","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.23140000000000002,0.23800000000000002,"0.300",0.0067,"Mercedes-Benz: AMG GT 63 S E PERFORMANCE (coupe), AMG S 63 E PERFORMANCE, AMG SL 63 S E PERFORMANCE"]
[2025,"Mitsubishi Motors Co","SMTXT01.5G5P","SMTXR0135A2A","MITSUBISHI","ECLIPSE CROSS ES 2WD","EB18-NE2A",6,1.499,3307,4630,3625,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N","JMTX10049245","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.169,0.21,"0.3000",0.041,"Mitsubishi Motors Corporation: ECLIPSE CROSS 2WD, ECLIPSE CROSS 4WD, ECLIPSE CROSS ES 2WD, ECLIPSE CROSS ES 4WD"]
[2025,"Nissan","SNSXT03.5PTC","SNSXR0201PEA","NISSAN","PATHFINDER 4WD PLATINUM","GRB122",0,3.5,4669,6062,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","NNSX10067654","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"NISSAN: PATHFINDER 2WD, PATHFINDER 4WD"]
[2025,"Nissan","SNSXT03.5PTC","SNSXR0201PFB","NISSAN","PATHFINDER 4WD PLATINUM","GRB122",0,3.5,4669,6062,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","NNSX10067706","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.014400000000000001,0.014,"0.020",0,"NISSAN: PATHFINDER 4WD, PATHFINDER 4WD PLATINUM"]
[2025,"Porsche","SPRXT03.0CV6","SPRXR0176RED","Porsche","Cayenne","EC-9YA-AT-24",0,3,4837,6217,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","RPRX10079773","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.194,0.20800000000000002,"0.450",0.014,"Porsche: Cayenne, Cayenne Coupe"]
[2025,"Porsche","SPRXT04.0CV8","SPRXR0176RED","Porsche","Cayenne","EC-9YA-AT-24",0,3,4837,6217,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","RPRX10079775","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Porsche: Cayenne Turbo GT"]
[2025,"Porsche","SPRXV04.0R92","SPRXR0170R92","Porsche","911 Carrera Cabriolet","FE-992-25",0,3,3620,4442,4000,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"N","SPRX10086627","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.224,0.224,"0.300",0,"Porsche: 911 GT3 RS"]
[2025,"Subaru","SFJXV02.4AJM","SFJXR01165AC","SUBARU","BRZ","NBV-MZ42",0,2.4,2903,3748,3250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","NFJX10068289","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17830000000000001,0.184,"0.300",0.0061,"Subaru: BRZ  TOYOTA: GR86"]
[2025,"Toyota","STYXT02.0P3H","STYXR0130P72","TOYOTA","CAMRY XLE/XSE","18-AV1A",1,2.487,3415,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","JTYX10046336","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.012100000000000001,0.012,"0.020",0,"TOYOTA: COROLLA CROSS, COROLLA CROSS AWD"]
[2025,"Toyota","STYXT02.5H3A","STYXR0195J82","TOYOTA","SIENNA AWD","21-AL1H",1,2.487,4860,6170,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","NTYX10069935","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.153,0.153,"0.400",0,"TOYOTA: SIENNA, SIENNA AWD"]
[2025,"Toyota","STYXT03.4M53","STYXR0170J92","TOYOTA","4RUNNER 4WD","25-TN2H",0,2.3930000000000002,5310,6505,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","STYX10085722","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.03,0.03,"0.20",0,"LEXUS: LX 700h"]
[2025,"Toyota","STYXV01.6B5A","STYXR0130P72","TOYOTA","CAMRY","18-AV1A",2,2.487,3425,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","NTYX10068444","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.26880000000000004,0.269,"0.300",0,"TOYOTA: GR COROLLA"]
[2025,"Toyota","STYXV02.5P34","STYXR0165J72","LEXUS","RX 500h AWD","23-TL1H",0,2.3930000000000002,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"Y","PTYX10075331","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1549,0.155,"0.300",0,"TOYOTA: TOYOTA CROWN AWD"]
[2025,"Toyota","STYXV03.5M5A","STYXR0165P72","LEXUS","IS 300","21-AC1A",0,1.998,3805,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MTYX10065255","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",5.5000000000000005E-3,0.006,"0.020",0,"LEXUS: IS 300 AWD, IS 350, IS 350 AWD, RC 300 AWD, RC 350, RC 350 AWD"]
[2025,"Volkswagen Group of","SVGAJ01.5V2L","SVGAR0139VEP","Volkswagen","Taos 4Motion","VW316550191",0,1.498,3538,4608,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","SVGA91006012","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1714,0.171,"0.275",0,"Volkswagen: Taos, Taos 4Motion"]
[2025,"Volkswagen Group of","SVGAJ03.0N7N","SVGAR0182NCM","Audi","Q7","RA77-Q7-452",0,2,5049,6393,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","RVGA10080555","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Audi: Q7, Q8 quattro"]
[2025,"Volkswagen Group of","SVGAT02.0A77","SVGAR0182NCM","Audi","Q7","RA77-Q7-452",0,2,5049,6393,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","RVGA10080552","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.009000000000000001,0.02,"0.20",0.007,"Audi: Q7"]
[2025,"Volkswagen Group of","SVGAV02.0A7N","SVGAR0139ACB","Audi","A3 quattro","NA3B-A3-531",0,1.984,3527,4475,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"Y","NVGA10070352","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.23900000000000002,0.23900000000000002,"0.275",0,"Audi: S3"]
[2025,"Volkswagen Group of","SVGAV04.0P7B","SVGAR0180P7B","Porsche","Panamera Turbo PHEV","EVAP-972TH-25",0,4,5481,6239,6000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","SPRX10087694","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC",2E-3,0.01,"0.20",0.005,"Bentley: Continental GT, Continental GT Speed, Continental GTC, Continental GTC Speed, Flying Spur, Flying Spur Speed"]
[2025,"Volvo","SVVXJ02.0U70","SVVXR0107E64","Volvo","XC40 B5 AWD","202320",0,1.969,3934,4895,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PVVX10074518","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,1E-3,"0.050",0,"Volvo Cars of North America, LLC: XC40 B5 AWD"]
[2024,"aston martin","RASXJ04.0AEX","RASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065542","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Aston Martin Lagonda Ltd: DBX 707, DBX V8"]
[2024,"BMW","RBMXJ02.0B4X","RBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe, X3 sDrive30i, X3 xDrive30i, X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2024,"BMW","RBMXJ03.0H70","RBMXR0180G7H","BMW","X5 xDrive50e","9N02303",0,3,5573,7055,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","RBMX10078643","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"BMW: 750e xDrive Sedan"]
[2024,"BMW","RBMXT02.0U1X","RBMXR0120U11","BMW","X1 xDrive28i","5U31827",0,2,3750,4850,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","PBMX10075680","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.013000000000000001,0.01,"0.02",0,"BMW: X1 M35i, X2 M35i"]
[2024,"BMW","RBMXT04.4S6M","RBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063966","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.05,"0.20",0.011000000000000001,"BMW: X5 M Competition, X6 M Competition"]
[2024,"BMW","RBMXV02.0M48","RBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17170000000000002,0.219,"0.300",0.047400000000000005,"BMW: 230i Coupe, 230i xDrive Coupe"]
[2024,"BMW","RBMXV04.4SM5","RBMXR0150G1X","BMX","M8 Competition Gran Coupe","BT81619",0,4.4,4480,5380,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NBMX10067265","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.009000000000000001,0.01,"0.02",0,"BMW: M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2024,"FCA US LLC","RCRXD06.45V2","RCRXF0273TP0","RAM","2500 4X4","L1DJ76370",0,6.4,8500,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MCRX10066902","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.6214000000000001,0.627,"0.725",0.0057,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2024,"FCA US LLC","RCRXD06.45W5","RCRXF0275TP0","RAM","3500 Cab Chassis 4X4","L1DD82812",0,6.4,11251,13500,11500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","NCRX10075816","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0187,0.019,"0.030",0,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2024,"FCA US LLC","RCRXD06.45W5","RCRXR0380TP1","RAM","3500 Cab Chassis 4X4","L1DD82811",0,6.4,11251,13500,11500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MCRX10075710","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.024900000000000002,0.025,"0.030",0,"RAM: 3500 4X2, 3500 4X4"]
[2024,"FCA US LLC","RCRXT02.05PH","RCRXR0180FEH","Jeep","Grand Cherokee 4xe","L2WLX8854",0,2,5396,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","NCRX10071605","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Grand Cherokee 4xe"]
[2024,"FCA US LLC","RCRXT03.05P2","RCRXR0230RP0","Jeep","Grand Wagoneer L 4x4","L3WSJ8111",0,3,6619,8000,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10075664","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.334,0.34,"0.550",0.0057,"Jeep: Grand Wagoneer L 4x4"]
[2024,"FCA US LLC","RCRXT03.65P5","RCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.038,0.04,"0.20",0,"Jeep: Gladiator 4X4"]
[2024,"FCA US LLC","RCRXT03.65PH","RCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045056","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24180000000000001,0.248,"0.450",0.0057,"Chrysler: Pacifica Hybrid"]
[2024,"FCA US LLC","RCRXT05.75P0","RCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059603","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2024,"FCA US LLC","RCRXT06.4CP1","RCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Dodge: Durango SRT AWD"]
[2024,"FCA US LLC","RCRXT06.4FP1","RCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX91004326","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.35550000000000004,0.36100000000000004,"0.500",0.0057,"Dodge: Durango SRT AWD"]
[2024,"FOMOCO","RFMXD03.56BG","RFMXF0215GDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-448",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061753","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0,0,"1.0",0,"Ford: TRANSIT T250 CHASSIS CAB 2WD FFV, TRANSIT T250 CHASSIS CAB 4WD FFV, TRANSIT T250 CUTAWAY 2WD FFV, TRANSIT T250 CUTAWAY 4WD FFV, TRANSIT T350 CHASSIS CAB 2WD FFV, TRANSIT T350 CHASSIS CAB 4WD FFV, TRANSIT T350 CUTAWAY 2WD FFV, TRANSIT T350 CUTAWAY 4WD FFV"]
[2024,"FOMOCO","RFMXD03.56BZ","RFMXF0215GDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-448",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060460","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: TRANSIT T250 CHASSIS CAB 2WD, TRANSIT T250 CHASSIS CAB 4WD, TRANSIT T250 CUTAWAY 2WD, TRANSIT T250 CUTAWAY 4WD, TRANSIT T350 CHASSIS CAB 2WD, TRANSIT T350 CHASSIS CAB 4WD, TRANSIT T350 CUTAWAY 2WD, TRANSIT T350 CUTAWAY 4WD"]
[2024,"FOMOCO","RFMXD03.57BZ","RFMXF0185NDJ","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",0,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060474","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.3E-3,0.003,"0.030",0,"Ford: TRANSIT T350 CHASSIS CAB 2WD, TRANSIT T350 CHASSIS CAB 4WD, TRANSIT T350 CUTAWAY 2WD, TRANSIT T350 CUTAWAY 4WD"]
[2024,"FOMOCO","RFMXD06.87BC","RFMXR0250NHJ","Ford","F350 4x4","LFE1-6.2-571",0,6.2,8742,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061482","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: F250 PICKUP 2WD FFV, F250 PICKUP 4WD FFV, F350 PICKUP 2WD FFV, F350 PICKUP 4WD FFV"]
[2024,"FOMOCO","RFMXD07.363H","RFMXR0360NHJ","Ford","F350 4x4","LFE1-6.2-J-578",0,6.2,9000,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061061","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.3774,0.377,"0.600",0,"Ford: F250 PICKUP 2WD, F250 PICKUP 4WD"]
[2024,"FOMOCO","RFMXT02.02Y2","RFMXR0125GDF","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",3.8E-3,0.004,"0.020",0,"Ford: BRONCO SPORT 4WD, MAVERICK AWD, MAVERICK FWD"]
[2024,"FOMOCO","RFMXT02.31EM","RFMXR0140NDF","Ford","Bronco","MG11-2.3-J-203",0,2.3000000000000003,5136,6120,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","MFMX10067812","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.098,0.1,"000.20",2E-3,"Ford: BRONCO 4WD, BRONCO BADLANDS 4WD, BRONCO BLACK DIAMOND 4WD, BRONCO SASQUATCH 4WD"]
[2024,"FOMOCO","RFMXT02.52B2","RFMXR0135LDF","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Ford: MAVERICK HEV FWD"]
[2024,"FOMOCO","RFMXT03.03V7","RFMXR0140NDG","Ford","Bronco","MG11-2.3-J-203",0,2.3000000000000003,5136,6120,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","MFMX10067818","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: BRONCO RAPTOR 4WD"]
[2024,"FOMOCO","RFMXT03.33U3","RFMXR0185NDG","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"000.20",1E-3,"Ford: INTERCEPTOR UTILITY AWD FFV"]
[2024,"FOMOCO","RFMXV05.0VKN","RFMXR0130NDE","Ford","Mustang","PZJ1-5.0-J-660",0,5,4113,4860,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","RFMX10078669","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"000.05",0,"Ford: MUSTANG, MUSTANG DARK HORSE"]
[2024,"GM","RGMXD06.6170","RGMXF019060C","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","66GDMET947",0,6.6000000000000005,10455,12300,11500,"R","2-Wheel Drive, Rear","A","Automatic","A6",6,"Y","N",null,null,"N","PGMX10075105","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4481,0.448,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2024,"GM","RGMXD06.6230","RGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2024,"GM","RGMXT02.0550","RGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061440","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.29150000000000004,0.29200000000000004,"0.450",0,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2024,"GM","RGMXT02.7100","RGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10054575","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0083,0.008,"0.020",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2024,"GM","RGMXT06.2376","RGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053898","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1998,0.2,"0.500",0,"Cadillac: ESCALADE V AWD"]
[2024,"GM","RGMXV01.5010","RGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10060943","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2111,0.21100000000000002,"0.300",0,"Chevrolet: MALIBU"]
[2024,"GM","RGMXV03.6043","RGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10060942","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Cadillac: CT4 V, CT5, CT5 AWD, CT5 V, CT5 V AWD"]
[2024,"Honda","RHNXT01.5MWC","RHNXR0122BBA","HONDA","CR-V AWD","EP8A3C",0,1.5,3640,4795,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","PHNX10074499","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.011000000000000001,0.02,"0.20",0.01,"Honda: CR-V FWD"]
[2024,"Honda","RHNXT03.53TC","RHNXR0150BAA","HONDA","ODYSSEY FWD","EHMR3A",0,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10046192","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.10650000000000001,0.10600000000000001,"0.400",null,"Honda: PASSPORT AWD, RIDGELINE AWD, RIDGELINE AWD TrailSport"]
[2024,"Honda","RHNXT03.5CCC","RHNXR0150BAA","HONDA","ODYSSEY FWD","EHMR3A",0,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10046191","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.12290000000000001,0.12300000000000001,"0.400",null,"Acura: MDX AWD, MDX FWD"]
[2024,"Honda","RHNXV01.5SDC","RHNXR0122ABA","ACURA","INTEGRA","ERPV2M",0,2,3253,3957,3500,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N","RHNX10078634","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.051000000000000004,0.06,"0.20",0.01,"Honda: CIVIC 4Dr"]
[2024,"Honda","RHNXV02.07EB","RHNXR0122AAA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044436","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Honda: ACCORD, ACCORD SPORT/TOURING"]
[2024,"Hyundai","RHYXT01.6L13","RHYXR0135L1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064839","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"HYUNDAI MOTOR COMPANY: Tucson Hybrid, Tucson Hybrid Blue"]
[2024,"Hyundai","RHYXT02.5LR3","RHYXR0125LRG","HYUNDAI","Tucson","NX4U1H5GA095A",0,2.5,3647,4861,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NHYX10066722","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.267,0.267,"0.300",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2024,"Hyundai","RHYXT02.5TP5","RHYXR0162TTG","Genesis","GV80","JX-U1L5TA205A",1,3.5,5004,6108,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NHYX10068789","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1983,0.198,"0.400",0,"GENESIS: GV80 AWD, GV80 RWD"]
[2024,"Hyundai","RHYXV01.6M13","RHYXR0137M1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064837","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"HYUNDAI MOTOR COMPANY: Santa Fe Hybrid AWD, Santa Fe Hybrid FWD"]
[2024,"Hyundai","RHYXV01.6SB5","RHYXR0120SBG","HYUNDAI","Venue","QX-U0G6MC120F",0,1.6,2737,3770,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LHYX10058709","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"HYUNDAI MOTOR COMPANY: Venue"]
[2024,"Hyundai","RHYXV02.5GP4","RHYXR0132GPG","Genesis","G80","RG3U1L5TA082A",0,3.5,4497,5567,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX10062527","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",0,"GENESIS: G70 AWD, G70 RWD"]
[2024,"Hyundai","RHYXV02.5HP5","RHYXR0142HTG","Genesis","G80","RG3U1L5TA082A",0,3.5,4497,5567,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX10062528","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0148,0.015000000000000001,"0.020",0,"GENESIS: G80 AWD, G80 RWD"]
[2024,"Hyundai","RHYXV03.5HT5","RHYXR0142HTG","Genesis","G80","RG3U1L5TA082A",0,3.5,4497,5567,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX91004651","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.20720000000000002,0.20700000000000002,"0.300",0,"GENESIS: G80 AWD"]
[2024,"Jaguar Land Rover L","RJLXJ05.0FSM","RJLXR0140P1Z","Land Rover","Range Rover Evoque","3EVPP037",0,2,3995,5181,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","EJLX10039802","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0176,0.018000000000000002,"0.020",0,"Jaguar: F-PACE SVR"]
[2024,"Jaguar Land Rover L","RJLXT02.0RTW","RJLXR0175P1B","LAND ROVER","New Range Rover","3KMVP032",0,4.4,5705,7385,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NJLX10072657","MFR","24","Federal fuel refueling test (ORVR)","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","120","HC",0.004,0,"0.20",0,"Land Rover: Defender 110, Defender 90"]
[2024,"Jaguar Land Rover L","RJLXT05.0FSN","RJLXR0175P1B","LAND ROVER","New Range Rover","3KMVP032",0,4.4,5705,7385,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NJLX10072655","MFR","24","Federal fuel refueling test (ORVR)","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.07300000000000001,0.07,"0.20",0,"Land Rover: Defender 110, Defender 90"]
[2024,"Kia","RKMXT01.6P13","RKMXR0135P1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064841","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.03,0.03,"0.20",0,"KIA: Sportage Hybrid AWD, Sportage Hybrid FWD"]
[2024,"Kia","RKMXT02.5JP3","RKMXR0144JPG","Kia","Sorento","MQ4U1H5GA042A",0,2.5,3935,5467,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10065283","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.20",0.003,"KIA: Sorento AWD, Sorento FWD"]
[2024,"Kia","RKMXT03.8ML4","RKMXR0135MLG","KIA","Telluride","ON-U0L8GA003A",0,3.8000000000000003,4299,5736,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LKMX10056260","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.021,0.02,"0.20",2E-3,"KIA: Telluride AWD, Telluride FWD"]
[2024,"Kia","RKMXV01.6DC5","RKMXR0133DCG","Kia","K5","DL3U1G6TA007F",0,1.6,3115,4354,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10062912","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.004,0,"0.05",0,"KIA: K5, K5 AWD"]
[2024,"Lotus","RLTXV03.5JHB","RLTXR0130JHB","Lotus","Emira","EDV-24-EVSA6",0,3.5,3241,3902,3625,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"N","N",null,null,"N","RLTX10082875","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.011000000000000001,0.01,"0.02",0,"Lotus Cars Ltd: Emira"]
[2024,"Maserati","RMAXJ03.0TJI","RMAXR0150189","Maserati","Granturismo Trofeo","380671",0,3,4072,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","RMAX10076952","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1627,0.168,"0.300",0.0057,"MASERATI: Grancabrio Trofeo, Granturismo Modena, Granturismo Trofeo"]
[2024,"MAZDA","RTKXT02.5CDA","RTKXR0117GCQ","MAZDA","CX-5","7EFPYS1-032",0,2.5,3527,4515,3875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HTKX10045490","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.014100000000000001,0.014,"0.020",0,"MAZDA: CX-5 4WD"]
[2024,"MAZDA","RTKXV02.5EGA","RTKXR0098ADP","MAZDA","MAZDA3","1EBPYTG1-001",2,2.5,3383,4299,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","MTKX10064912","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1759,0.20800000000000002,"0.300",0.032600000000000004,"MAZDA: CX-30 4WD, MAZDA3 4-Door 4WD, MAZDA3 5-Door 4WD"]
[2024,"Mercedes-Benz","RMBXJ02.0HY2","RMBXR0095LNA","Mercedes-Benz","AMG GLB 35 4MATIC","X247E20DETC-Z2128",2,1.991,4114,5430,4500,"F","2-Wheel Drive, Front","AM","Automated Manual",null,8,"Y","N",null,null,"N","NMBX91004809","EPA","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.29450000000000004,0.29400000000000004,"0.300",0,"Mercedes-Benz: CLA 250, CLA 250 4MATIC, GLA 250, GLA 250 4MATIC"]
[2024,"Mercedes-Benz","RMBXT04.0HY2","RMBXR0170LNC","Mercedes-Benz","GLS 580 4MATIC","X167E40DETC-Z2030",4,3.982,5828,7480,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"Y","MMBX10068820","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.36100000000000004,0.36100000000000004,"0.475",0,"Mercedes-Benz: AMG GLE 63 S 4MATIC+, AMG GLE 63 S 4MATIC+ (coupe)"]
[2024,"Mercedes-Benz","RMBXT04.0U2C","RMBXR0170LNC","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10048076","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.017400000000000002,0.017,"0.020",0,"Mercedes-Benz: AMG G 63 4x4 Squared"]
[2024,"Mercedes-Benz","RMBXV02.0HY5","RMBXR0160LNP","Mercedes-Benz","S 580e 4MATIC","V223E30DETC-Z2304",0,2.999,5813,6768,6000,"A","All Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","PMBX10078678","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Mercedes-Benz: AMG C 63 S E Performance"]
[2024,"Mercedes-Benz","RMBXV03.0HY3","RMBXR0140LNC","Mercedes-Benz","C 300 4MATIC","W206E20DETC-Z2306",1,1.999,4019,5148,4250,"A","All Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","PMBX10076512","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",2E-3,0,"0.05",0,"Mercedes-Benz: CLE 450 4MATIC (Convertible), CLE 450 4MATIC (Coupe), E 450 4MATIC AT (station wagon)"]
[2024,"Mercedes-Benz","RMBXV04.0HY1","RMBXR0170LNZ","Mercedes-Benz","S 580 4MATIC","V223E40DETC-Z2148",0,3.982,4942,6210,5250,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","MMBX10068170","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.008,0.008,"0.020",0,"Mercedes-Benz: S 580 4MATIC Maybach"]
[2024,"Mercedes-Benz","RMBXV04.0U3A","RMBXR0170LNE","Mercedes-Benz","AMG SL 55 4MATIC+","R232E40DETC-Z2225",0,3.982,4330,5115,4750,"A","All Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","NMBX10074703","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.336,0.336,"0.375",0,"Mercedes-Benz: AMG GT 55 4MATIC+ (coupe), AMG GT 63 4MATIC+ (coupe), AMG SL 55 4MATIC+, AMG SL 63 4MATIC+"]
[2024,"Nissan","RNSXT01.5A3C","RNSXR0128PEA","NISSAN","ROGUE AWD SL/PLATINUM SL","CTB527",0,1.5,3707,4685,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","MNSX10067315","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24500000000000002,0.24500000000000002,"0.375",0,"NISSAN: ROGUE AWD, ROGUE AWD SL/PLATINUM, ROGUE FWD, ROGUE FWD SL/PLATINUM"]
[2024,"Nissan","RNSXT02.5APA","RNSXR0105PEA","NISSAN","ROGUE AWD SV/SL/PLATINUM PLATINUM","CTB157",0,2.5,3645,4619,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","MNSX91004630","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1705,0.17,"0.400",0,"MITSUBISHI MOTORS: Outlander 4WD"]
[2024,"Nissan","RNSXT05.6P9B","RNSXR0201PFA","NISSAN","TITAN 4WD PRO-4X","TVC364",0,5.6000000000000005,5855,7300,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","JNSX10051386","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0115,0.012,"0.020",0,"INFINITI: QX80 2WD, QX80 4WD  NISSAN: ARMADA 2WD, ARMADA 4WD"]
[2024,"Nissan","RNSXV03.0PXA","RNSXR0159MCC","NISSAN","Z SPORT","FGB745",0,3,3610,4211,4000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","PNSX10071521","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.21080000000000002,0.21100000000000002,"0.300",0,"NISSAN: Z, Z NISMO"]
[2024,"Nissan","RNSXV03.0PXA","RNSXR0159MCC","NISSAN","Z SPORT","FGB745",0,3,3610,4211,4000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","PNSX10071528","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.265,0.265,"0.300",0,"NISSAN: Z, Z NISMO"]
[2024,"Porsche","RPRXT04.0CV8","RPRXR0176RED","Porsche","Cayenne","EC-9YA-AT-24",0,3,4837,6217,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","RPRX10079772","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2209,0.232,"0.450",0.0108,"Porsche: Cayenne S, Cayenne S Coupe, Cayenne Turbo GT"]
[2024,"Porsche","RPRXV03.0C92","RPRXR0170R92","Porsche","911 Carrera S","EC-992S-PDK-20",0,3,3382,4376,3875,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"N","MPRX10065419","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Porsche: 911 Carrera, 911 Carrera 4, 911 Carrera 4 Cabriolet, 911 Carrera 4 GTS, 911 Carrera 4 GTS Cabriolet, 911 Carrera 4S, 911 Carrera 4S Cabriolet, 911 Carrera Cabriolet, 911 Carrera GTS, 911 Carrera GTS Cabriolet, 911 Carrera S, 911 Carrera S Cabriolet, 911 Carrera T, 911 Dakar, 911 Targa 4, 911 Targa 4 GTS, 911 Targa 4S"]
[2024,"Subaru","RFJXJ02.5BUY","RFJXR01435DB","SUBARU","OUTBACK AWD","LBV-YB16",0,2.5,3757,4850,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N","LFJX10057039","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.19340000000000002,0.193,"0.300",0,"Subaru: LEGACY, OUTBACK AWD"]
[2024,"Subaru","RFJXT02.4SAF","RFJXR01535HF","SUBARU","ASCENT LIMITED/TOURING","KBV-AE192",0,2.4,4608,6000,5000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N","KFJX10051148","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Subaru: ASCENT AWD, ASCENT LIMITED/TOURING/ONYX EDITION AWD"]
[2024,"Toyota","RTYXJ02.4P3G","RTYXR0130P72","TOYOTA","CAMRY","18-AV1A",2,2.487,3425,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","NTYX10068443","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"LEXUS: NX 350 AWD, NX 350 AWD F SPORT"]
[2024,"Toyota","RTYXT02.4P3R","RTYXR0165P82","TOYOTA","SIENNA AWD","17-GL4A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","HTYX10041720","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.005,0,"0.20",0,"TOYOTA: TACOMA 2WD, TACOMA 4WD, TACOMA SR5/SPORT/OFFROAD/LIMITED 4WD, TACOMA SR5/SPORT/PRERUNNER 2WD"]
[2024,"Toyota","RTYXT02.5N4M","RTYXR0130P82","TOYOTA","NX 250 AWD","22-AZ2A",0,2.487,3790,4995,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","NTYX10069839","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.20",0,"LEXUS: NX 250, NX 250 AWD"]
[2024,"Toyota","RTYXT03.4M5W","RTYXR0215P92","TOYOTA","TUNDRA 4WD","22-VK3A",1,3.4450000000000003,5665,7310,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","NTYX10071224","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.03,0.03,"0.20",0,"TOYOTA: TUNDRA 2WD, TUNDRA 4WD"]
[2024,"Toyota","RTYXT03.5P33","RTYXR0165J92","LEXUS","TX 550h+ AWD","24-GU2H",0,3.456,5400,6540,5500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"N","N",null,null,"Y","RTYX10082003","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"LEXUS: TX 550h+ AWD"]
[2024,"Toyota","RTYXV02.0P3B","RTYXR0130J72","TOYOTA","COROLLA HYBRID AWD","23-ZE2H",0,1.798,3265,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","PTYX10074891","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1608,0.161,"0.300",0,"LEXUS: UX 250h, UX 250h AWD"]
[2024,"Volkswagen Group of","RVGAJ01.5V3Q","RVGAR0139VCF","VOLKSWAGEN","Taos","VW316-51-0428",0,1.498,3199,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","NVGA10068549","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.225,0.24,"0.275",0.0151,"Volkswagen: Taos, Taos 4Motion"]
[2024,"Volkswagen Group of","RVGAJ02.0A7G","RVGAR0155ACN","Audi","Q5","PA7E-Q5-244",0,2,4167,5379,4750,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"Y","PVGA10074047","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.308,0.308,"0.400",0,"Audi: Q5 S line quattro, Q5 Sportback S line quattro"]
[2024,"Volkswagen Group of","RVGAJ03.0N7F","RVGAR0155ACP","Audi","A4 Allroad quattro 55 TFSI","PA7G-A4-402",1,2,3957,5016,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"Y","PVGA10074269","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.185,0.185,"0.300",0,"Audi: RS 5 Coupe, RS 5 Sportback, S4, S5 Cabriolet, S5 Coupe, S5 Sportback"]
[2024,"Volkswagen Group of","RVGAJ04.0NAT","RVGAR0182NCM","Audi","Q7","RA77-Q7-452",0,2,5049,6393,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","RVGA10080553","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.311,0.322,"0.450",0.011000000000000001,"Audi: RS Q8"]
[2024,"Volkswagen Group of","RVGAT02.0A77","RVGAR0182NCM","Audi","Q7","RA77-Q7-452",0,2,5049,6393,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","RVGA10080552","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.009000000000000001,0.02,"0.20",0.007,"Audi: Q7 quattro"]
[2024,"Volkswagen Group of","RVGAV02.0V7B","RVGAR0139VCA","Volkswagen","GTI","VW38003-0082",0,1.984,3316,4343,3750,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"N","PVGA10074777","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.012,0.012,"0.020",0,"Volkswagen: GTI, Golf R"]
[2024,"Volkswagen Group of","RVGAV05.2NDE","RVGAR0155NCL","AUDI","R8","LNBE-R8B",2,5.204000000000001,3968,null,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LVGA10058208","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.341,0.35400000000000004,"0.500",0.013000000000000001,"Lamborghini: Huracan Coupe 2WD, Huracan Spyder, Huracan Sterrato"]
[2024,"Volvo","RVVXJ02.0U70","RVVXR0142E50","Volvo","XC60 B5 AWD","202216",0,1.969,4204,5400,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","NVVX10069711","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0099,0.01,"0.020",0,"Volvo Cars of North America, LLC: XC90 B5 AWD"]
[2023,"aston martin","PASXJ04.0AEX","PASXR0160T3B","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","MASX10065519","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.02,0,"0.2",6.3E-3,"Aston Martin Lagonda Ltd: DBX 707, DBX V8"]
[2023,"BMW","PBMXJ02.0B4X","PBMXR0130F60","Mini","COOPER COUNTRYMAN ALL4","3L07920",2,1.5,3643,4564,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NBMX10067486","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.152,0.161,"0.300",0.0088,"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2023,"BMW","PBMXJ04.4N63","PBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064491","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.05",0,"BMW: X5 M50i, X6 M50i"]
[2023,"BMW","PBMXJ04.4SM5","PBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10064376","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1961,0.226,"0.500",0.0297,"BMW: X5 M, X5 M Competition, X6 M, X6 M Competition"]
[2023,"BMW","PBMXV01.5B36","PBMXR0100F5X","Mini","Mini Cooper (5-doors)","T826907",0,1.5,2815,3750,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FBMX10033195","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.269,0.273,"0.300",0.0037,"Mini: COOPER CONVERTIBLE, COOPER HARDTOP 2 DOOR, COOPER HARDTOP 4 DOOR"]
[2023,"BMW","PBMXV02.0M48","PBMXR0130F60","Mini","COOPER COUNTRYMAN ALL4","3L07920",1,1.5,3643,4564,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MBMX10064486","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.007,0.01,"0.02",0,"BMW: M235i xDrive Gran Coupe, X2 M35i  Mini: JCW COUNTRYMAN ALL4, JOHN COOPER WORKS CLUBMAN ALL4"]
[2023,"BMW","PBMXV03.0B5X","PBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044979","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2179,0.226,"0.300",0.0081,"BMW: M240i Coupe, M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2023,"FCA US LLC","PCRXD06.45W5","PCRXF0275TP0","RAM","3500 Cab Chassis 4X4","L1DD82812",0,6.4,11251,13500,11500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","NCRX10069064","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.6321,0.641,"0.725",0.009000000000000001,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2023,"FCA US LLC","PCRXD06.45W5","PCRXR0380TP1","RAM","2500 Cab Chassis 4X4","L0DJ79243",1,6.4,9000,10000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MCRX10067046","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 3500 4X2, 3500 4X4"]
[2023,"FCA US LLC","PCRXT02.05P1","PCRXR0115PP3","Jeep","Compass 4X4","L3MPJ2067",0,2,3620,4800,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10076922","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"ALFA ROMEO: Tonale AWD  Dodge: Hornet AWD"]
[2023,"FCA US LLC","PCRXT02.45P1","PCRXR0118PP0","Jeep","Cherokee 4X4","V4KLJ4101",0,2.4,3467,4612,3750,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10043875","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.026000000000000002,0.03,"0.20",0,"Jeep: Cherokee 4X4"]
[2023,"FCA US LLC","PCRXT03.05P1","PCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Jeep: Wagoneer 4x2, Wagoneer 4x4"]
[2023,"FCA US LLC","PCRXT03.65P1","PCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049481","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3013,0.31,"0.500",0.009000000000000001,"RAM: 1500 Classic 4X2, 1500 Classic 4X4"]
[2023,"FCA US LLC","PCRXT03.65P2","PCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044755","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.045000000000000005,0.04,"0.20",0,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2023,"FCA US LLC","PCRXT03.65P5","PCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10074149","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015000000000000001,0.015000000000000001,"0.020",0,"Jeep: Gladiator 4X4"]
[2023,"FCA US LLC","PCRXT03.65P7","PCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044760","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34700000000000003,0.35300000000000004,"0.450",0.0057,"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2023,"FCA US LLC","PCRXT03.65P9","PCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 4dr 4X4"]
[2023,"FCA US LLC","PCRXT05.75P0","PCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10073747","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0129,0.013000000000000001,"0.020",0,"Dodge: Durango AWD, Durango Pursuit AWD, Durango RWD"]
[2023,"FCA US LLC","PCRXT06.4CP1","PCRXR0172RP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.600",0.0057,"Jeep: Wrangler 4dr 4X4"]
[2023,"FCA US LLC","PCRXV06.25PA","PCRXR0168PPA","Dodge","Challenger SRT Demon 170","L3LAD8815",0,6.2,4405,5450,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","PCRX10081147","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.369,0.375,"0.500",0.0057,"Dodge: Challenger SRT Demon 170"]
[2023,"FCA US LLC","PCRXV06.2FP0","PCRXR0168PP0","Dodge","Challenger Widebody","L2LAD4459",0,6.4,4288,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","NCRX10071116","MFR","24","Federal fuel refueling test (ORVR)","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.1,0.1,"0.20",0,"Dodge: Challenger SRT, Challenger SRT Widebody, Charger SRT Widebody"]
[2023,"Ferrari","PFEXV03.9TUR","PFEXR0175149","Ferrari","F8 Spider","243588",0,3.9,3626,4281,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","MFEX10068577","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.2189,0.219,"0.300",0,"Ferrari North America, Inc.: F8 Spider, F8 Tributo"]
[2023,"FOMOCO","PFMXD03.56BZ","PFMXF0185NDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061754","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0,0,"1.0",0,"Ford: TRANSIT T250 CHASSIS CAB 2WD, TRANSIT T250 CHASSIS CAB 4WD, TRANSIT T250 CUTAWAY 2WD, TRANSIT T250 CUTAWAY 4WD, TRANSIT T350 CHASSIS CAB 2WD, TRANSIT T350 CHASSIS CAB 4WD, TRANSIT T350 CUTAWAY 2WD, TRANSIT T350 CUTAWAY 4WD"]
[2023,"FOMOCO","PFMXD03.57BG","PFMXR0215GDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-448",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060451","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.20220000000000002,0.202,"0.600",0,"Ford: TRANSIT T350 VAN 2WD FFV, TRANSIT T350 WAGON 2WD FFV"]
[2023,"FOMOCO","PFMXD03.57BZ","PFMXR0215GDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-448",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060460","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: TRANSIT T350 VAN 2WD, TRANSIT T350 VAN 4WD, TRANSIT T350 WAGON 2WD, TRANSIT T350 WAGON 4WD"]
[2023,"FOMOCO","PFMXD07.373K","PFMXR0360NHJ","Ford","F350 4x4","LFE1-6.2-J-578",0,6.2,9000,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061062","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: F250 PICKUP 2WD, F250 PICKUP 4WD, F350 PICKUP 2WD, F350 PICKUP 4WD"]
[2023,"FOMOCO","PFMXT02.02JU","PFMXR0135NDF","Lincoln","Nautilus","KD92-2.7-H-192",0,2.7,4744,5960,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KFMX10053375","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1441,0.14400000000000002,"0.400",0,"Ford: EDGE AWD, EDGE FWD  Lincoln: NAUTILUS AWD, NAUTILUS FWD"]
[2023,"FOMOCO","PFMXT02.31EM","PFMXR0140NDG","Ford","Bronco","MG11-2.3-J-203",0,2.3000000000000003,5136,6120,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","MFMX10067818","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"000.05",0,"Ford: BRONCO 4WD, BRONCO BADLANDS 4WD, BRONCO BLACK DIAMOND 4WD, BRONCO SASQUATCH 4WD"]
[2023,"FOMOCO","PFMXT02.53CE","PFMXR0135LLN","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063695","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","T3","Federal Tier 3 Evap","150","OMHCE",0,0,"0.05",0,"Lincoln: CORSAIR AWD PHEV"]
[2023,"FOMOCO","PFMXT02.72V6","PFMXR0140NDG","Ford","Bronco","MG11-2.3-J-203",0,2.3000000000000003,5136,6120,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","MFMX10067818","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"000.05",0,"Ford: BRONCO 4WD, BRONCO BADLANDS 4WD, BRONCO SASQUATCH 4WD"]
[2023,"FOMOCO","PFMXT03.33U3","PFMXR0185NDG","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060896","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.016,0.02,"000.05",0,"Ford: INTERCEPTOR UTILITY AWD FFV"]
[2023,"FOMOCO","PFMXT03.54JM","PFMXR0260NDG","Ford","F-150","JFC1-2.7-J-027",0,2.7,4903,7000,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047783","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.25370000000000004,0.254,"0.500",0,"Ford: F150 PICKUP TREMOR 4WD, F150 RAPTOR 4WD"]
[2023,"GM","PGMXD04.3392","PGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2023,"GM","PGMXD06.6394","PGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064689","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3388,0.339,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: G3500 SAVANA 2WD CUTAWAY CH, SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2023,"GM","PGMXD06.6398","PGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064692","MFR","15","Spitback","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.24,0.2,"1.0",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH, SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS, SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH, SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS, SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2023,"GM","PGMXT02.7100","PGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10054575","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0083,0.008,"0.020",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES  GMC: SIERRA 2WD, SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES"]
[2023,"GM","PGMXT05.3386","PGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055636","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4646,0.465,"0.525",0,"Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2023,"GM","PGMXV01.3545","PGMXR01023BB","BUICK","ENCORE GX FWD","1250N023GC",0,1.2,3039,null,3375,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"N","LGMX91004525","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.158,0.158,"0.300",0,"Buick: ENCORE GX AWD, ENCORE GX FWD  Chevrolet: TRAILBLAZER AWD, TRAILBLAZER FWD"]
[2023,"GM","PGMXV03.6043","PGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10060943","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2111,0.21100000000000002,"0.300",0,"Cadillac: CT4 V, CT5, CT5 AWD, CT5 V, CT5 V AWD"]
[2023,"GM","PGMXV06.2089","PGMXR013030B","CADILLAC","CTS AWD","206GAE4665",0,2,3947,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JGMX10051643","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.017,0.017,"0.020",0,"Chevrolet: CAMARO"]
[2023,"Honda","PHNXT03.0HTC","PHNXR0150CBA","ACURA","RDX AWD A-SPEC","EKYF4A",0,2,4087,5027,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KHNX10052116","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.011000000000000001,0.01,"0.20",0,"Acura: MDX AWD Type-S"]
[2023,"Honda","PHNXT03.5RSC","PHNXR0150BAA","HONDA","ODYSSEY FWD","EHMR3A",0,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10046192","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.10650000000000001,0.10600000000000001,"0.400",null,"Honda: PASSPORT AWD, PASSPORT FWD, RIDGELINE AWD, RIDGELINE FWD"]
[2023,"Honda","PHNXV02.07EB","PHNXR0122AAA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044298","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0044,0.004,"0.020",0,"Honda: ACCORD, ACCORD SPORT/TOURING"]
[2023,"Honda","PHNXV02.0FEC","PHNXR0122AAA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044435","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2016,0.202,"0.300",0,"Honda: CIVIC 5Dr"]
[2023,"Hyundai","PHYXT01.6M13","PHYXR0137M1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064837","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"HYUNDAI MOTOR COMPANY: Santa Fe Hybrid, Santa Fe Hybrid Blue"]
[2023,"Hyundai","PHYXT02.5MP5","PHYXR0144MPG","Kia","Sorento","MQ4U1H5GA042A",0,2.5,3935,5467,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10065285","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"HYUNDAI MOTOR COMPANY: Santa Fe AWD, Santa Fe FWD"]
[2023,"Hyundai","PHYXT02.5TP5","PHYXR0162TTG","Genesis","GV80","JX-U1L5TA205A",1,3.5,5004,6108,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NHYX10068818","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.134,0.13,"0.20",0,"GENESIS: GV80 AWD, GV80 RWD"]
[2023,"Hyundai","PHYXV01.6CC5","PHYXR0130CCG","HYUNDAI","Elantra","CN7U1G6TD143F",0,1.6,3020,3990,3375,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","MHYX10065352","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"HYUNDAI MOTOR COMPANY: Elantra"]
[2023,"Hyundai","PHYXV01.6SB5","PHYXR0120SBG","HYUNDAI","Venue","QX-U0G6MC120F",0,1.6,2737,3770,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LHYX10058703","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.21300000000000002,0.21300000000000002,"0.300",0,"HYUNDAI MOTOR COMPANY: Venue"]
[2023,"Hyundai","PHYXV02.0CE5","PHYXR0130CEG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038647","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0056,0.006,"0.020",0,"HYUNDAI MOTOR COMPANY: Elantra"]
[2023,"Hyundai","PHYXV02.0GG6","PHYXR0132GGG","Hyundai","Sonata","DN8U0G6TA019F",0,1.6,3336,4354,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LHYX91004413","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.184,0.184,"0.300",0,"GENESIS: G70 AWD, G70 RWD"]
[2023,"Hyundai","PHYXV02.5HP5","PHYXR0142HTG","Genesis","G80","RG3U1L5TA082A",0,3.5,4497,5567,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX10062680","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"GENESIS: G80 AWD, G80 RWD"]
[2023,"Hyundai","PHYXV03.3GK6","PHYXR0132GKG","Kia","Sorento","UM9L3AU01AC",0,3.3000000000000003,4303,5622,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KKMX10050518","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.014,0.02,"0.20",2E-3,"GENESIS: G70 AWD, G70 RWD"]
[2023,"Jaguar Land Rover L","PJLXJ02.0RTX","PJLXR0160P1Z","Jaguar","XJ","2DFLVP35",0,3,4287,5235,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","FJLX10031805","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.007,0.01,"0.20",0,"Jaguar: XF P250, XF P250 AWD, XF P300 AWD"]
[2023,"Jaguar Land Rover L","PJLXT02.0RTF","PJLXR0140P1Z","Land Rover","Range Rover Evoque","3EVPP037",0,2,3995,5181,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","EJLX10028181","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2268,0.227,"0.400",0,"Jaguar: E-PACE MHEV  Land Rover: Range Rover Evoque MHEV"]
[2023,"Jaguar Land Rover L","PJLXT04.4GTE","PJLXR0175P1B","LAND ROVER","New Range Rover","3KMVP032",0,4.4,5705,7385,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NJLX10072640","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.322,0.322,"0.500",0,"Land Rover: New Range Rover, New Range Rover LWB, New Range Rover Sport"]
[2023,"Kia","PKMXT01.6NC5","PKMXR0125NCG","KIA","SELTOS","SP2U1G6T364A",0,1.6,3317,4245,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","NKMX10066952","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"KIA: Seltos AWD"]
[2023,"Kia","PKMXT02.5JP5","PKMXR0144JPG","Kia","Sorento","MQ4U1H5GA042A",0,2.5,3935,5467,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10065283","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.20",0.003,"KIA: Sorento AWD, Sorento FWD"]
[2023,"Kia","PKMXT03.8ML5","PKMXR0135MLG","KIA","Telluride","ON-U0L8GA003A",0,3.8000000000000003,4299,5736,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LKMX10056264","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"KIA: Telluride AWD, Telluride FWD"]
[2023,"Kia","PKMXV01.6AB6","PKMXR0110ABG","KIA","Rio","SC9R6GU11AC",0,1.6,2727,3616,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LKMX10055984","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.01,0.01,"0.20",2E-3,"KIA: Rio"]
[2023,"Kia","PKMXV01.6J13","PKMXR0137J1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064840","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24180000000000001,0.24200000000000002,"0.300",0,"KIA: Sorento Hybrid AWD, Sorento Hybrid FWD"]
[2023,"Kia","PKMXV02.5DP5","PKMXR0133DPG","Hyundai","Sonata","DN8U0H5GA023F",0,2.5,3120,4354,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LHYX10059890","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.18580000000000002,0.186,"0.300",0,"KIA: K5"]
[2023,"Kia","PKMXV03.3EK6","PKMXR0132EKG","Kia","Sorento","UM9L3AU01AC",0,3.3000000000000003,4303,5622,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KKMX10050518","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.014,0.02,"0.20",2E-3,"KIA: Stinger AWD, Stinger RWD"]
[2023,"MAZDA","PTKXT02.5EGB","PTKXR0117GAQ","MAZDA","CX-5","2EBPYTS1-004",0,2.5,3699,4718,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","NTKX10070976","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"MAZDA: CX-5 4WD"]
[2023,"MAZDA","PTKXV02.5CDB","PTKXR0098GDP","MAZDA","Mazda3","9DBPYUDS1-001",0,2.5,3091,4069,3375,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","KTKX10055246","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","B","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",null,"MAZDA: CX-30 4WD"]
[2023,"Mercedes-Benz","PMBXJ02.0U3A","PMBXR0155LNC","Mercedes-Benz","AMG GLC 43 4MATIC","X253E30DETC-Z2011",3,2.996,4324,5420,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N","MMBX10069129","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.274,0.274,"0.275",0,"Mercedes-Benz: C 300 (Coupe), C 300 (convertible), C 300 4MATIC (Coupe), C 300 4MATIC (convertible), E 350, E 350 4MATIC, GLC 300 4MATIC (Coupe)"]
[2023,"Mercedes-Benz","PMBXJ04.0U2A","PMBXR0155LNA","Mercedes-Benz","AMG C 63 S (coupe)","C205E40DETC-Z2130",0,3.982,4155,4860,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N","MMBX10068863","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1668,0.167,"0.375",0,"Mercedes-Benz: AMG C 63 S (convertible), AMG C 63 S (coupe), AMG E 63 S 4MATIC+, AMG E 63 S 4MATIC+ (SW), AMG GT 63 4MATIC+, AMG GT 63 S 4MATIC+"]
[2023,"Mercedes-Benz","PMBXT04.0HY2","PMBXR0170LNC","Mercedes-Benz","GLS 580 4MATIC","X167E40DETC-Z2030",4,3.982,5828,7480,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"Y","MMBX10066454","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Mercedes-Benz: AMG GLE 63 S 4MATIC+, AMG GLE 63 S 4MATIC+ (coupe), AMG GLS 63 4MATIC+, GLS 600 4MATIC Maybach"]
[2023,"Mercedes-Benz","PMBXV02.0HY2","PMBXR0140LNA","Mercedes-Benz","AMG C 43 4MATIC","W206E20DETC-Z2307",0,1.991,4238,5181,4500,"A","All Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","PMBX10077649","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Mercedes-Benz: AMG C 43 4MATIC"]
[2023,"Mercedes-Benz","PMBXV02.0U3B","PMBXR0095LNB","Mercedes-Benz","AMG CLA 45 4MATIC+","C118E20DETC-Z2019",2,1.991,3719,4729,4000,"4","4-Wheel Drive","AM","Automated Manual",null,8,"Y","N",null,null,"N","LMBX10065608","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Mercedes-Benz: AMG CLA 45 4MATIC, AMG GLA 45 4MATIC"]
[2023,"Mitsubishi Motors Co","PMTXT02.4G5P","PMTXR0135A2D","MITSUBISHI","LANCER","EB17-CA8A",3,1.998,3003,3969,3250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)","AV-S6(w / Paddles ; 6-speed)",6,"Y","N",null,null,"N","HMTX10039872","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.13,0.13,"0.3000",0,"Mitsubishi Motors Corporation: Outlander Sport 2WD, Outlander Sport 4WD, RVR 2WD, RVR 4WD"]
[2023,"Nissan","PNSXD05.6W9A","PNSXF0201PHA","NISSAN","TITAN XD 4WD PRO-4X","TVC784",0,5.6000000000000005,6691,8730,7500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","NNSX10070744","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3109,0.311,"0.600",0,"NISSAN: TITAN XD 4WD"]
[2023,"Nissan","PNSXT01.5A3C","PNSXR0128PDA","NISSAN","ROGUE AWD SL/PLATINUM SL","CTB527",0,1.5,3707,4685,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","MNSX10067355","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0057,0.006,"0.020",0,"NISSAN: ROGUE FWD"]
[2023,"Nissan","PNSXT03.5PTD","PNSXR0201PFB","NISSAN","PATHFINDER 4WD PLATINUM","GRB122",0,3.5,4669,6062,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","NNSX10067642","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1647,0.165,"0.500",0,"INFINITI: QX60 AWD, QX60 FWD  NISSAN: PATHFINDER 4WD ROCK CREEK"]
[2023,"Nissan","PNSXT05.6P9A","PNSXR0201PFA","NISSAN","TITAN 4WD PRO-4X","TVC364",0,5.6000000000000005,5855,7300,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","JNSX10050859","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2862,0.28600000000000003,"0.500",0,"NISSAN: TITAN 2WD, TITAN 4WD, TITAN 4WD PRO-4X"]
[2023,"Nissan","PNSXV02.5RPB","PNSXR0114PCB","NISSAN","ALTIMA SR/PLATINUM","FRB170",0,2.5,3443,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","KNSX10053965","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"NISSAN: ALTIMA, ALTIMA AWD, ALTIMA AWD SL/SR, ALTIMA AWD SR/PLATINUM, ALTIMA SL/SR, ALTIMA SV"]
[2023,"Nissan","PNSXV03.0PXA","PNSXR0159MCC","NISSAN","Z SPORT","FGB745",0,3,3610,4211,4000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","PNSX10071521","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.21080000000000002,0.21100000000000002,"0.300",0,"NISSAN: Z"]
[2023,"Porsche","PPRXT03.0CV6","PPRXR0170RMA","Porsche","Macan","EC-95BII-22",0,2,4151,5534,4500,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","NPRX10071621","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0.003,"Porsche: Macan GTS, Macan S"]
[2023,"Porsche","PPRXV02.9PV6","PPRXR0190RP7","Porsche","Panamera 4S","EC-971S-20",0,2.9,4414,5501,4750,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"N","LPRX10060352","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.183,0.183,"0.300",0,"Porsche: Panamera, Panamera 4, Panamera 4 Executive, Panamera 4 ST, Panamera 4S, Panamera 4S Executive, Panamera 4S ST"]
[2023,"Porsche","PPRXV04.0PV8","PPRXR0190RP7","Porsche","Panamera 4S","EC-971S-20",0,2.9,4414,5501,4750,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"N","LPRX10060359","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",1E-3,"Porsche: Panamera GTS, Panamera GTS ST, Panamera Turbo S, Panamera Turbo S Executive, Panamera Turbo S ST"]
[2023,"Porsche","PPRXV04.0S92","PPRXR0170R92","Porsche","911 Carrera S","EC-992S-PDK-20",0,3,3382,4376,3875,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"N","MPRX10065417","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.300",0,"Porsche: 911 GT3, 911 GT3 Touring"]
[2023,"Subaru","PFJXT02.0EVC","PFJXR01485JG","SUBARU","CROSSTREK","KBV-CG193",0,2,3766,4901,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","KFJX91003939","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1802,0.18,"0.400",0,"Subaru: CROSSTREK HYBRID AWD"]
[2023,"Subaru","PFJXV02.4CZA","PFJXR01545GA","SUBARU","WRX","NBV-AV14",1,2.4,3576,4620,3875,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N","NFJX10070013","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.003,0,"0.20",1E-3,"Subaru: WRX"]
[2023,"Toyota","PTYXT02.5P33","PTYXR0165J82","TOYOTA","RAV4 PRIME AWD","21-AP2H",1,2.487,4300,5530,4500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","NTYX10070413","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.23240000000000002,0.232,"0.400",0,"LEXUS: NX 450h+ AWD  TOYOTA: RAV4 PRIME AWD"]
[2023,"Toyota","PTYXT02.5P34","PTYXR0195J82","TOYOTA","SIENNA AWD","21-AL1H",0,2.487,4825,6170,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","MTYX10065380","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",0,"TOYOTA: SIENNA, SIENNA AWD"]
[2023,"Toyota","PTYXV01.8P33","PTYXR0130J72","TOYOTA","PRIUS PRIME","17-ZW3H",0,1.798,3365,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HTYX10042567","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC",1E-3,0,"0.20",0,"TOYOTA: COROLLA HYBRID, COROLLA HYBRID AWD"]
[2023,"Toyota","PTYXV02.0P3C","PTYXR0130P72","TOYOTA","CAMRY","18-AV1A",2,2.487,3425,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","NTYX10068443","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"TOYOTA: COROLLA, COROLLA HATCHBACK, COROLLA HATCHBACK XSE"]
[2023,"Toyota","PTYXV03.5M5B","PTYXR0130P72","TOYOTA","CAMRY","18-AV1A",2,2.487,3425,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","NTYX10068444","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.26880000000000004,0.269,"0.300",0,"LEXUS: ES 350, ES 350 F SPORT  TOYOTA: CAMRY, CAMRY TRD, CAMRY XSE"]
[2023,"Volkswagen Group of","PVGAJ02.0A7G","PVGAR0150NCS","AUDI","A8L","KN7M-D5",0,2.995,4806,null,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KVGA10055598","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.014,0.04,"0.20",0.025,"Audi: A6 quattro"]
[2023,"Volkswagen Group of","PVGAJ02.0V3A","PVGAR0135ACT","VOLKSWAGEN","Tiguan","UTI017",0,1.984,3885,5247,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVGA10048151","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.323,0.323,"0.350",0,"Volkswagen: Tiguan, Tiguan 4Motion, Tiguan R-Line 4Motion, Tiguan S"]
[2023,"Volkswagen Group of","PVGAJ04.0NAT","PVGAR0150NCS","AUDI","A8L","KN7M-D5",0,2.995,4806,null,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KVGA10055599","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.14300000000000002,0.155,"0.300",0.012,"Audi: RS 6 Avant, RS 7"]
[2023,"Volkswagen Group of","PVGAT03.0NAQ","PVGAR0155NCV","BENTLEY","Bentayga","BY636/2_28881",0,2.995,5844,null,6000,"A","All Wheel Drive","A","Automatic",null,8,"Y","N",null,null,"Y","MVGA10067710","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.21100000000000002,0.227,"0.500",0.016,"Bentley: Bentayga Hybrid"]
[2023,"Volkswagen Group of","PVGAT04.0NAV","PVGAR0150NCM","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX91004097","EPA","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2225,0.234,"0.450",0.011000000000000001,"Audi: SQ7, SQ8"]
[2023,"Volkswagen Group of","PVGAV02.5NAG","PVGAR0139NCB","Audi","RS3","NNAG-RS3",0,2.48,3671,4608,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","NVGA10073279","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0.005,"0.050",0.003,"Audi: RS3"]
[2023,"Volkswagen Group of","PVGAV05.2NDE","PVGAR0155NCL","AUDI","R8","LNBE-R8B",2,5.204000000000001,3968,null,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LVGA10058209","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.005,0.01,"0.20",0.006,"Lamborghini: Huracan Coupe, Huracan Coupe 2WD, Huracan Spyder, Huracan Spyder 2WD"]
[2023,"Volvo","PVVXJ02.0U70","PVVXR0107E64","Volvo","XC40 B5 AWD","202320",0,1.969,3934,4895,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","PVVX10074518","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,1E-3,"0.050",0,"Volvo Cars of North America, LLC: XC40 B4 AWD, XC40 B5 AWD"]
[2023,"Volvo","PVVXJ02.0U70","PVVXR0142E54","Volvo","XC60 B5 AWD","202216",0,1.969,4204,5400,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","NVVX10069713","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,1E-3,"0.050",0,"Volvo Cars of North America, LLC: V60CC B5 AWD, XC60 B5 AWD"]
[2022,"BMW","NBMXJ02.0B4X","NBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: 330i Sedan, 330i xDrive Sedan, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 530i Sedan, 530i xDrive Sedan, X3 sDrive30i, X3 xDrive30i, X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2022,"BMW","NBMXJ04.4SM5","NBMXR0150G1X","BMX","M8 Competition Gran Coupe","BT81619",0,4.4,4480,5380,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","NBMX10067261","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.011000000000000001,0.01,"0.05",0,"BMW: M5 CS Sedan, M5 Competition Sedan, M5 Sedan, M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe"]
[2022,"BMW","NBMXT03.0H05","NBMXR0170H05","BMW","X5 xDrive45e","LE48301",0,3,5646,6967,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","MBMX10063096","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.006,0.01,"0.20",2E-3,"BMW: X5 xDrive45e"]
[2022,"BMW","NBMXV02.0M48","NBMXR0130F60","Mini","COOPER COUNTRYMAN ALL4","3L07920",1,1.5,3643,4564,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MBMX10064485","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","4","HC-TOTAL-EQUIV",0.0051,0.005,"0.020",0,"BMW: M235i xDrive Gran Coupe, X2 M35i  Mini: JCW COUNTRYMAN ALL4, JOHN COOPER WORKS CLUBMAN ALL4"]
[2022,"BMW","NBMXV03.0B5X","NBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: M240i xDrive Coupe, Z4 M40i  TOYOTA: Supra 3.0"]
[2022,"BMW","NBMXV03.0SM3","NBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045186","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.17170000000000002,0.195,"0.300",0.023700000000000002,"BMW: M3 Competition M xDrive Sedan, M3 Competition Sedan, M3 Sedan, M4 Competition Coupe, M4 Competition M xDrive Coupe, M4 Coupe, M4CompetitionMxDriveConvertible"]
[2022,"FCA US LLC","NCRXD06.45W5","NCRXR0380TP1","RAM","2500 Cab Chassis 4X4","L0DJ79243",1,6.4,9000,10000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MCRX10067034","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4872,0.49300000000000005,"0.700",0.0057,"RAM: 3500 4X2, 3500 4X4, 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2022,"FCA US LLC","NCRXJ02.95P0","NCRXR0112PP1","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048786","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.18460000000000001,0.194,"0.400",0.009000000000000001,"ALFA ROMEO: Stelvio AWD"]
[2022,"FCA US LLC","NCRXT01.35P0","NCRXR0110PP1","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043878","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2566,0.262,"0.325",0.0057,"Jeep: Renegade Trailhawk 4x4"]
[2022,"FCA US LLC","NCRXT03.05P2","NCRXR0204RP1","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.023,0.02,"0.20",0,"Jeep: Grand Wagoneer 4x2, Grand Wagoneer 4x4"]
[2022,"FCA US LLC","NCRXT03.65P1","NCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049483","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.03,0.03,"0.20",0,"RAM: 1500 Classic 4X2, 1500 Classic 4X4"]
[2022,"FCA US LLC","NCRXT03.65P7","NCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2022,"FCA US LLC","NCRXT03.65P8","NCRXR0166RP1","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Gladiator 4X4"]
[2022,"FCA US LLC","NCRXT03.65P9","NCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 2dr 4X4"]
[2022,"FCA US LLC","NCRXT05.75P2","NCRXR0225RP1","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049390","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.036000000000000004,0.04,"0.20",0,"RAM: 1500 Classic 4X2, 1500 Classic 4X4"]
[2022,"FCA US LLC","NCRXT06.4FP1","NCRXR0204RP1","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059604","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3297,0.339,"0.500",0.009000000000000001,"Jeep: Grand Wagoneer 4x2, Grand Wagoneer 4x4"]
[2022,"Ferrari","NFEXV03.9HYB","NFEXR017508H","Ferrari","SF90 Spider","242405",0,3.9,4145,4683,4500,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"Y","NFEX10067548","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.28,0.3,"0.3",0,"Ferrari North America, Inc.: SF90 Spider, SF90 Stradale"]
[2022,"Ferrari","NFEXV03.9T50","NFEXR017508K","Ferrari","Portofino M","229643",0,3.9,3759,4859,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"N","N",null,null,"N","MFEX10062926","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.019,0.02,"0.02",0,"Ferrari North America, Inc.: Portofino M, Roma"]
[2022,"FOMOCO","NFMXD03.56BZ","NFMXF0215GDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-448",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060451","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.20220000000000002,0.202,"0.600",0,"Ford: TRANSIT T250 CHASSIS CAB 2WD, TRANSIT T250 CHASSIS CAB 4WD, TRANSIT T250 CUTAWAY 2WD, TRANSIT T250 CUTAWAY 4WD, TRANSIT T350 CHASSIS CAB 2WD, TRANSIT T350 CHASSIS CAB 4WD, TRANSIT T350 CUTAWAY 2WD, TRANSIT T350 CUTAWAY 4WD"]
[2022,"FOMOCO","NFMXD06.26BC","NFMXF0360NHJ","Ford","F350 4x4","LFE1-6.2-J-578",0,6.2,9000,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10065864","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.010100000000000001,0.01,"0.030",0,"Ford: F250 2WD BED DELETE FFV, F250 4WD BED DELETE FFV, F350 2WD BED DELETE FFV, F350 4WD BED DELETE FFV"]
[2022,"FOMOCO","NFMXD06.27BC","NFMXF0250NDJ","Ford","F350 4x4","LFE1-6.2-571",0,6.2,8742,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061480","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3521,0.35200000000000004,"0.600",0,"Ford: F350 2WD BED DELETE FFV, F350 4WD BED DELETE FFV"]
[2022,"FOMOCO","NFMXD07.373K","NFMXR0360NHJ","Ford","F350 4x4","LFE1-6.2-J-578",0,6.2,9000,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10065864","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.010100000000000001,0.01,"0.030",0,"Ford: F350 2WD, F350 4WD"]
[2022,"FOMOCO","NFMXT02.02JU","NFMXR0135NDF","Lincoln","Nautilus","KD92-2.7-H-192",0,2.7,4744,5960,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KFMX10053377","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: EDGE AWD, EDGE FWD  Lincoln: NAUTILUS AWD, NAUTILUS FWD"]
[2022,"FOMOCO","NFMXT02.31EM","NFMXR0140NDG","Ford","Bronco","MG11-2.3-J-203",0,2.3000000000000003,5136,6120,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","MFMX10068292","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.37260000000000004,0.373,"000.500",0,"Ford: BRONCO 4WD, BRONCO BADLANDS 4WD, BRONCO BLACK DIAMOND 4WD, BRONCO SASQUATCH 4WD"]
[2022,"FOMOCO","NFMXT02.36HG","NFMXR0135NDG","Ford","Ranger - Chassis Cab","KFG1-2.3-H-367",0,2.3000000000000003,4527,6050,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KFMX10055550","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.010700000000000001,0.011000000000000001,"0.020",0,"Ford: RANGER 2WD, RANGER 4WD"]
[2022,"FOMOCO","NFMXT02.52P1","NFMXR0135LLN","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10060716","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.006,0.01,"0.20",0,"Ford: ESCAPE FWD PHEV"]
[2022,"FOMOCO","NFMXT03.03V7","NFMXR0140NDG","Ford","Bronco","MG11-2.3-J-203",0,2.3000000000000003,5136,6120,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","MFMX10068292","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.37260000000000004,0.373,"000.500",0,"Ford: BRONCO RAPTOR 4WD"]
[2022,"FOMOCO","NFMXT03.33U3","NFMXR0185NDF","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060895","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2015,0.202,"0.400",0,"Ford: EXPLORER FFV AWD"]
[2022,"FOMOCO","NFMXT03.54JK","NFMXR0260NDG","Ford","F-150","JFC1-2.7-J-027",0,2.7,4903,7000,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047785","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2022,"FOMOCO","NFMXV03.5VGT","NFMXR0130NKE","Ford","GT","LGX1-3.5-J-858",0,3.5,3379,3779,3625,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"Y","N",null,null,"N","LFMX10061980","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.004,0.01,"000.20",0.005,"Ford: FORD GT"]
[2022,"GM","NGMXD04.3392","NGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064545","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.39990000000000003,0.4,"0.600",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD PASS  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2022,"GM","NGMXD06.6378","NGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCMET996",0,4.3,6400,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064546","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.053000000000000005,0.05,"0.20",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD, SILVERADO 3500 HD 2WD, SILVERADO 3500 HD 4WD  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD, SIERRA 3500 HD 2WD, SIERRA 3500 HD 4WD"]
[2022,"GM","NGMXT02.0500","NGMXR009537C","CHEVROLET","EQUINOX","151JXV5723",0,1.5,3543,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","JGMX10046505","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1645,0.164,"0.375",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2022,"GM","NGMXT03.6151","NGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040173","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.33390000000000003,0.334,"0.450",0,"Buick: ENCLAVE AWD, ENCLAVE FWD  Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD, TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2022,"GM","NGMXT06.2375","NGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053898","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1998,0.2,"0.500",0,"Cadillac: ESCALADE 2WD, ESCALADE 4WD  Chevrolet: SILVERADO 4WD, SILVERADO 4WD MUD TERRAIN TIRES, SILVERADO 4WD ZR2, TAHOE 2WD, TAHOE 4WD  GMC: SIERRA 4WD, SIERRA 4WD MUD TERRAIN TIRES, YUKON 2WD, YUKON 4WD"]
[2022,"GM","NGMXV01.4001","NGMXR011230A","BUICK","ENCORE FWD","143SV986DA",0,1.4000000000000001,3195,null,3500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","MGMX10065639","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Buick: ENCORE AWD, ENCORE FWD  Chevrolet: TRAX AWD, TRAX FWD"]
[2022,"GM","NGMXV02.0031","NGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10061522","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.009000000000000001,0.009000000000000001,"0.020",0,"Chevrolet: MALIBU"]
[2022,"GM","NGMXV06.2094","NGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10060942","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Cadillac: CT5 V"]
[2022,"Honda","NHNXT01.5YLC","NHNXR01221SA","HONDA","CR-V 1.5L TC","EHPA2C",0,1.5,3562,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044431","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Honda: CR-V AWD, CR-V FWD"]
[2022,"Honda","NHNXV01.5CEB","NHNXR0155VSA","HONDA","INSIGHT","EKL22C",0,1.5,3051,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y","KHNX10052131","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1105,0.11,"0.300",0,"Honda: INSIGHT, INSIGHT TOURING"]
[2022,"Honda","NHNXV02.0AEC","NHNXR0149VSA","ACURA","RDX AWD A-SPEC","EKYF4A",0,2,4087,5027,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KHNX10052116","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.011000000000000001,0.01,"0.20",0,"Acura: TLX AWD, TLX AWD A-SPEC, TLX FWD, TLX FWD A-SPEC"]
[2022,"Honda","NHNXV02.0BEB","NHNXR0122VSA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044435","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2016,0.202,"0.300",0,"Honda: ACCORD, ACCORD SPORT/TOURING"]
[2022,"Hyundai","NHYXT01.6L13","NHYXR0135L1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064840","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24180000000000001,0.24200000000000002,"0.400",0,"HYUNDAI MOTOR COMPANY: Tucson Hybrid, Tucson Hybrid Blue"]
[2022,"Hyundai","NHYXT01.6M13","NHYXR0137M1G","KIA","SORENTO HYBRID","MQ4U1G6HA581F",0,1.6,4065,5578,4250,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y","MKMX10064840","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24180000000000001,0.24200000000000002,"0.400",0,"HYUNDAI MOTOR COMPANY: Santa Fe Hybrid, Santa Fe Hybrid Blue"]
[2022,"Hyundai","NHYXT02.5VR5","NHYXR0145VRG","Kia","Sorento","MQ4U1H5GA042A",0,2.5,3935,5467,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10065285","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"HYUNDAI MOTOR COMPANY: Santa Cruz AWD, Santa Cruz FWD"]
[2022,"Hyundai","NHYXT03.8NL5","NHYXR0135NLG","KIA","Telluride","ON-U0L8GA003A",0,3.8000000000000003,4299,5736,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LKMX10056262","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.017,0.02,"0.05",0.004,"HYUNDAI MOTOR COMPANY: Palisade AWD, Palisade FWD"]
[2022,"Hyundai","NHYXV01.6AB6","NHYXR0120ABG","KIA","Rio","SC9R6GU11AC",0,1.6,2727,3616,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LKMX91004119","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2551,0.255,"0.300",0,"HYUNDAI MOTOR COMPANY: Accent"]
[2022,"Hyundai","NHYXV01.6SB5","NHYXR0120SBG","HYUNDAI","Venue","QX-U0G6MC120F",0,1.6,2737,3770,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LHYX91004424","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24960000000000002,0.25,"0.300",0,"HYUNDAI MOTOR COMPANY: Venue"]
[2022,"Hyundai","NHYXV02.0CE3","NHYXR0130CEG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038646","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.028,0.03,"0.05",0,"HYUNDAI MOTOR COMPANY: Elantra"]
[2022,"Hyundai","NHYXV02.0KG6","NHYXR0125KGG","Hyundai","Kona","OS-U1G6TD127A",0,1.6,3287,4222,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","NHYX10067022","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"HYUNDAI MOTOR COMPANY: Kona N"]
[2022,"Hyundai","NHYXV02.5EP5","NHYXR0133EPG","Hyundai","Sonata","DN8U0H5GA023F",0,2.5,3120,4354,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LHYX10059886","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.006,0.01,"0.05",0,"HYUNDAI MOTOR COMPANY: Sonata"]
[2022,"Hyundai","NHYXV02.5UP5","NHYXR0142UPG","Genesis","G80","RG3U1L5TA082A",0,3.5,4497,5567,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX10062681","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.020",0,"GENESIS: GV70 AWD, GV70 RWD"]
[2022,"Jaguar Land Rover L","NJLXJ02.0RTX","NJLXR0160P1Z","Jaguar","XJ","2DFLVP35",0,3,4287,5235,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","FJLX10031801","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",1E-3,0,"0.05",0,"Jaguar: XF P250, XF P250 AWD, XF P300 AWD"]
[2022,"Jaguar Land Rover L","NJLXT02.0PTW","NJLXR0175M1A","LAND ROVER","Range Rover","LKJVP221",0,2,5915,6125,6000,"4","4-Wheel Drive","A","Automatic",null,1,"Y","N",null,null,"Y","KJLX10057219","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.01,0.01,"0.20",0,"Land Rover: Range Rover Sport PHEV"]
[2022,"Jaguar Land Rover L","NJLXT05.0FSN","NJLXR0175P1Z","LAND ROVER","LR4","SDV18",0,4.4,5649,6807,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","EJLX10024513","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","120","HC",0.014,0.01,"0.20",0,"Land Rover: Defender 110, Defender 90, Range Rover, Range Rover LWB, Range Rover LWB SVA, Range Rover SVA, Range Rover Sport, Range Rover Sport SVR"]
[2022,"Kia","NKMXT02.0HG5","NKMXR0133HGG","HYUNDAI","Tucson","TL6N0HU03AC",0,2,3489,4740,3750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GHYX10034918","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1709,0.171,"0.400",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FWD"]
[2022,"Kia","NKMXT02.4HH3","NKMXR0133HHG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10038257","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0112,0.011000000000000001,"0.020",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FWD"]
[2022,"Kia","NKMXT03.8ML5","NKMXR0135MLG","KIA","Telluride","ON-U0L8GA003A",0,3.8000000000000003,4299,5736,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LKMX10056261","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",6.8000000000000005E-3,0.007,"0.020",0,"KIA MOTORS CORPORATION: Telluride AWD, Telluride FWD"]
[2022,"Kia","NKMXV01.6BC5","NKMXR0114BCG","Kia","Soul","PS7N0AU01AC",0,2,3117,4101,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10041752","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.020",0,"KIA MOTORS CORPORATION: Soul"]
[2022,"Kia","NKMXV02.0BE3","NKMXR0114BEG","HYUNDAI","VELOSTER","JS9N0GU01AC",0,2,2844,3748,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","KHYX10050998","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.004,0.01,"0.05",0.003,"KIA MOTORS CORPORATION: Soul, Soul Eco dynamics"]
[2022,"Kia","NKMXV02.0CE3","NKMXR0130CEG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038644","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2555,0.256,"0.300",0,"KIA MOTORS CORPORATION: Forte, Forte 5, Forte FE"]
[2022,"Kia","NKMXV02.5DP5","NKMXR0133DPG","Hyundai","Sonata","DN8U0H5GA023F",0,2.5,3120,4354,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LHYX10059890","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.18580000000000002,0.186,"0.300",0,"KIA MOTORS CORPORATION: K5"]
[2022,"MAZDA","NTKXV02.0CDB","NTKXR0098GDP","MAZDA","Mazda3","9DBPYUDS1-001",0,2.5,3091,4069,3375,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","KTKX10055245","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","B","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2914,0.29100000000000004,"0.300",null,"MAZDA: CX-30 4WD, MAZDA3 4-Door 2WD, MAZDA3 5-Door 2WD"]
[2022,"McLaren Automotive ","NMLNV03.0M16","NMLNR0130M16","McLaren","Artura","SBM16AEA9KW990020",0,2.9930000000000003,3303,3871,3625,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"N","N",null,null,"Y","NMLN10070660","MFR","15","Spitback","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","SPITBACK",0.1,0.1,"1.0",0,"McLaren: Artura"]
[2022,"Mercedes-Benz","NMBXT02.0U3A","NMBXR0170LNF","Mercedes-Benz","GLE 350 4MATIC","V167E20DETC-Z2013",0,1.991,4853,6217,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N","LMBX10063292","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3285,0.328,"0.450",0,"Mercedes-Benz: GLE 350, GLE 350 4MATIC"]
[2022,"Mercedes-Benz","NMBXT03.0HY2","NMBXR0170LNF","Mercedes-Benz","GLE 350 4MATIC","V167E20DETC-Z2013",0,1.991,4853,6217,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N","LMBX10063089","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.013000000000000001,0.01,"0.20",0,"Mercedes-Benz: AMG GLE 53 4MATIC+, AMG GLE 53 4MATIC+ (coupe), GLE 450 4MATIC, GLE 450 4MATIC (coupe), GLS 450 4MATIC"]
[2022,"Mercedes-Benz","NMBXT04.0HY2","NMBXR0170LNC","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10048076","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.017400000000000002,0.017,"0.020",0,"Mercedes-Benz: AMG GLE 63 S 4MATIC+, AMG GLE 63 S 4MATIC+ (coupe), AMG GLS 63 4MATIC+, GLS 600 4MATIC Maybach"]
[2022,"Mercedes-Benz","NMBXV03.0HY3","NMBXR0170LND","Mercedes-Benz","S 580 4MATIC","V223E40DETC-Z2148",0,3.982,4942,6210,5250,"4","4-Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"Y","MMBX10068170","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.008,0.008,"0.020",0,"Mercedes-Benz: S 500, S 500 4MATIC, S 500 4MATIC (W)"]
[2022,"Mercedes-Benz","NMBXV04.0U3A","NMBXR0170LNE","Mercedes-Benz","AMG SL 55 4MATIC+","R232E40DETC-Z2225",0,3.982,4330,5115,4750,"A","All Wheel Drive","A","Automatic",null,9,"Y","N",null,null,"N","NMBX10074706","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.006,0.02,"0.20",0.016,"Mercedes-Benz: AMG SL 55 4MATIC+, AMG SL 63 4MATIC+"]
[2022,"Nissan","NNSXT01.5A3B","NNSXR0128PDA","NISSAN","ROGUE AWD SL/PLATINUM SL","CTB527",0,1.5,3707,4685,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","MNSX10067315","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24500000000000002,0.24500000000000002,"0.300",0,"NISSAN: ROGUE FWD"]
[2022,"Nissan","NNSXT02.5RPA","NNSXR0105PEA","NISSAN","ROGUE AWD SV/SL/PLATINUM PLATINUM","CTB157",0,2.5,3645,4619,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","MNSX10062634","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.194,0.194,"0.400",0,"MITSUBISHI MOTORS: Outlander 2WD"]
[2022,"Nissan","NNSXT02.5RPB","NNSXR0105PDA","NISSAN","ROGUE AWD SV/SL/PLATINUM PLATINUM","CTB157",1,2.5,3645,4619,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","MNSX10062630","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.07400000000000001,0.09,"0.20",0.019,"NISSAN: ROGUE FWD"]
[2022,"Nissan","NNSXT05.6P9A","NNSXR0201PFA","NISSAN","TITAN 4WD PRO-4X","TVC364",1,5.6000000000000005,5855,7300,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","JNSX10050855","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.08,0.08,"0.20",0,"NISSAN: TITAN 2WD, TITAN 4WD, TITAN 4WD PRO-4X"]
[2022,"Nissan","NNSXV03.0NHA","NNSXR0159MCB","INFINITI","Q50 AWD RED SPORT","HREH71",2,3,4025,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","JNSX10046122","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.01,0.01,"0.20",0,"INFINITI: Q50, Q50 AWD, Q50 AWD RED SPORT, Q50 RED SPORT, Q60, Q60 AWD, Q60 AWD RED SPORT, Q60 RED SPORT"]
[2022,"Porsche","NPRXT03.0CV6","NPRXR0170RMA","Porsche","Macan","EC-95BII-22",0,2,4151,5534,4500,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","NPRX10071621","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0.003,"Porsche: Macan GTS, Macan S"]
[2022,"Porsche","NPRXV02.9PH6","NPRXR0170RPH","Porsche","Panamera 4 e-Hybrid Executive","ECFE-971H-18",0,2.9,4960,6117,5500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","JPRX10048012","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1208,0.133,"0.300",0.0126,"Porsche: Panamera 4 E-Hybrid Executive, Panamera 4 E-Hybrid ST, Panamera 4 E-Hybrid/Exec/ST, Panamera 4S E-Hybrid Executive, Panamera 4S E-Hybrid ST, Panamera 4S E-Hybrid/Exec/ST"]
[2022,"Porsche","NPRXV04.0PH8","NPRXR0170RPH","Porsche","Panamera 4 e-Hybrid Executive","ECFE-971HA-18",0,2.9,4960,6117,5500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","JPRX10056031","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1812,0.198,"0.300",0.0164,"Porsche: Panamera Turbo S E-Hybrid Exec, Panamera Turbo S E-Hybrid ST, Panamera TurboS E-Hybrid/Exec/ST"]
[2022,"Subaru","NFJXJ02.4CZA","NFJXR01545GA","SUBARU","WRX","NBV-AV14",0,2.4,3576,4620,3875,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N","NFJX10070010","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1771,0.17700000000000002,"0.300",0,"Subaru: WRX"]
[2022,"Subaru","NFJXJ02.5BUY","NFJXR01545GE","SUBARU","CROSSTREK","JBV-YA195",0,2,3256,4343,3625,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N","JFJX10045962","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2184,0.22,"0.300",1.8000000000000002E-3,"Subaru: CROSSTREK AWD, FORESTER AWD, FORESTER WILDERNESS AWD"]
[2022,"Toyota","NTYXJ02.5N4L","NTYXR0130P72","TOYOTA","CAMRY","18-AV1A",2,2.487,3425,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","NTYX10068443","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"LEXUS: ES 250 AWD  TOYOTA: AVALON AWD, CAMRY AWD LE/SE, CAMRY AWD XLE/XSE, RAV4 AWD, RAV4 AWD LE, RAV4 AWD TRD OFFROAD"]
[2022,"Toyota","NTYXT02.5P3H","NTYXR0130P72","TOYOTA","CAMRY XLE/XSE","18-AV1A",1,2.487,3415,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","JTYX10046336","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.012100000000000001,0.012,"0.020",0,"TOYOTA: RAV4"]
[2022,"Toyota","NTYXT03.5M5M","NTYXR0165P82","TOYOTA","SIENNA AWD","17-GL4A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","HTYX10041743","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.23040000000000002,0.23,"0.400",0,"LEXUS: RX 350, RX 350 AWD, RX 350 L, RX 350 L AWD  TOYOTA: HIGHLANDER, HIGHLANDER AWD"]
[2022,"Toyota","NTYXV02.0M5A","NTYXR0165P72","LEXUS","IS 300","21-AC1A",0,1.998,3805,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MTYX10064706","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"LEXUS: IS 300, RC 300"]
[2022,"Toyota","NTYXV02.5P33","NTYXR0165J72","TOYOTA","CAMRY HYBRID XLE/SE","18-AV3H",0,2.487,3565,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","JTYX10047550","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.20",0,"LEXUS: ES 300h  TOYOTA: AVALON HYBRID, AVALON HYBRID XLE, CAMRY HYBRID LE, CAMRY HYBRID SE/XLE/XSE"]
[2022,"Toyota","NTYXV03.5M5C","NTYXR0180A72","LEXUS","LC 500","18-UZ2A",0,4.969,4280,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","JTYX10045648","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.007,0.01,"0.05",0,"LEXUS: LS 500, LS 500 AWD"]
[2022,"Volkswagen Group of","NVGAJ02.0A7G","NVGAR0140ACP","AUDI","A4","HAAC-BAQ",4,1.984,4035,null,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","HVGA10045302","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Audi: A4 S line quattro, A4 allroad quattro, A5 Cabriolet quattro, A5 Coupe quattro, A5 Sportback S line quattro"]
[2022,"Volkswagen Group of","NVGAJ02.0V3A","NVGAR0110VCA","AUDI","TT","UT-266/20",0,1.984,3450,null,3750,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LVGA10060291","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.256,0.256,"0.300",0,"Volkswagen: GLI"]
[2022,"Volkswagen Group of","NVGAJ03.0N7M","NVGAR0150NCS","AUDI","A6 Quattro (C8)","UC-412",0,1.984,4156,null,4500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"Y","KVGA10058954","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0164,0.016,"0.020",0,"Audi: A8 L quattro"]
[2022,"Volkswagen Group of","NVGAT04.0NAV","NVGAR0150NCM","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX10054422","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3559,0.37,"0.450",0.014,"Audi: SQ7, SQ8"]
[2022,"Volkswagen Group of","NVGAT06.0EAR","NVGAR0155ECR","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX91004097","EPA","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2225,0.234,"0.450",0.011000000000000001,"Bentley: Bentayga Speed"]
[2022,"Volkswagen Group of","NVGAV02.5NAG","NVGAR0139NCB","Audi","RS3","NNAG-RS3",0,2.48,3671,4608,4000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","NVGA10073277","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34,0.34900000000000003,"0.450",0.009000000000000001,"Audi: RS3"]
[2022,"Volkswagen Group of","NVGAV05.2NDE","NVGAR0155NCL","AUDI","R8","LNBE-R8B",2,5.204000000000001,3968,null,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LVGA10058208","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.341,0.35400000000000004,"0.500",0.013000000000000001,"Lamborghini: Huracan Coupe, Huracan Coupe RWD, Huracan Spyder, Huracan Spyder RWD"]
[2022,"Volvo","NVVXJ02.0S33","NVVXR0142E53","Volvo","XC60 B5 AWD","202216",0,1.969,4204,5400,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","NVVX10069711","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0099,0.01,"0.020",0,"Volvo Cars of North America, LLC: S90 B6 AWD"]
[2022,"Volvo","NVVXJ02.0U72","NVVXR0142E61","Volvo","XC40 T5 AWD","201923",0,1.969,3829,4895,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KVVX10051486","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.007,0.109,"0.200",0.10200000000000001,"Volvo Cars of North America, LLC: XC40 T4"]
[2022,"Volvo","NVVXJ02.0U73","NVVXR0142E53","Volvo","XC60 B5 AWD","202216",0,1.969,4204,5400,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","NVVX10069713","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",1E-3,1E-3,"0.050",0,"Volvo Cars of North America, LLC: S60 B5, S60 B5 AWD, XC60 B5"]
[2021,"BMW","MBMXJ03.0B07","MBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10045187","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe"]
[2021,"BMW","MBMXJ03.0H05","MBMXR0170H05","BMW","X5 xDrive45e","LE48301",0,3,5646,6967,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"Y","MBMX10063194","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.15230000000000002,0.167,"0.500",0.0143,"BMW: X5 xDrive45e"]
[2021,"BMW","MBMXT03.0G0X","MBMXR0180G05","BMW","X7 xDrive40i","L084470",0,3,5456,7022,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","MBMX10063966","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.043000000000000003,0.05,"0.20",0.006,"BMW: X5 sDrive40i, X5 xDrive40i, X6 sDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2021,"BMW","MBMXV01.5B36","MBMXR0130F60","Mini","COOPER COUNTRYMAN ALL4","3L07920",1,1.5,3643,4564,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MBMX10064488","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.14020000000000002,0.14,"0.300",0,"Mini: COOPER CLUBMAN ALL4, COOPER COUNTRYMAN, COOPER COUNTRYMAN ALL4"]
[2021,"BMW","MBMXV02.0M48","MBMXR0100F5X","Mini","Mini Cooper (5-doors)","T826907",0,1.5,2815,3750,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FBMX10033892","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",8.6E-3,0.009000000000000001,"0.020",0,"Mini: John Cooper Works GP"]
[2021,"FCA US LLC","MCRXD03.65V2","MCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060538","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1326,0.138,"0.550",0.0057,"RAM: Promaster 1500, Promaster 2500, Promaster 3500"]
[2021,"FCA US LLC","MCRXD06.45V4","MCRXF0273TP0","RAM","2500 4X4","L1DJ76370",0,6.4,8500,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MCRX10066902","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.6214000000000001,0.627,"0.800",0.0057,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2021,"FCA US LLC","MCRXT01.35P0","MCRXR0110PP0","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043879","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"FIAT: 500X AWD  Jeep: Renegade 4x2, Renegade 4x4"]
[2021,"FCA US LLC","MCRXT02.45P1","MCRXR0106PP1","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043880","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2414,0.25,"0.300",0.009000000000000001,"Jeep: Compass 4X4"]
[2021,"FCA US LLC","MCRXT02.45P1","MCRXR0106PP2","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017736","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.10600000000000001,0.11,"0.20",0,"Jeep: Compass 4X2"]
[2021,"FCA US LLC","MCRXT03.65P5","MCRXR0166PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Gladiator 4X4"]
[2021,"FCA US LLC","MCRXT03.65P7","MCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",0,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003702","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22190000000000001,0.228,"0.375",0.0057,"Jeep: Wrangler 2dr 4X4"]
[2021,"FCA US LLC","MCRXT03.65P8","MCRXR0204RP0","Dodge","Durango AWD","L0WDE8893",0,5.7,5427,7100,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10059606","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.023,0.02,"0.20",0,"Dodge: Durango AWD, Durango Pursuit AWD"]
[2021,"FCA US LLC","MCRXT05.75P1","MCRXR0225RP1","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049387","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4802,0.48900000000000005,"0.500",0.009000000000000001,"RAM: 1500 4X2, 1500 4X4"]
[2021,"FCA US LLC","MCRXT06.25P1","MCRXR0180RK0","Dodge","Durango SRT AWD","V9WDE4553",1,6.4,5512,7100,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10062648","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Dodge: Durango SRT AWD  Jeep: Grand Cherokee Trackhawk 4x4"]
[2021,"FCA US LLC","MCRXV05.75P3","MCRXR0168PP0","Dodge","Charger","L0LXC5442",0,5.7,4316,5300,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10062187","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.22360000000000002,0.229,"0.300",0.0057,"Chrysler: 300  Dodge: Challenger, Charger, Charger Pursuit"]
[2021,"Ferrari","MFEXV06.5GDI","MFEXR017512K","Ferrari","812 GTS","241041",0,6.5,4045,4687,4500,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","MFEX10062151","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.2541,0.254,"0.300",0,"Ferrari North America, Inc.: 812 GTS"]
[2021,"FOMOCO","MFMXD03.56BZ","MFMXR0185NDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060475","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.008,0.01,"0.20",1E-3,"Ford: TRANSIT T150 VAN 2WD, TRANSIT T150 VAN 4WD, TRANSIT T250 VAN 2WD, TRANSIT T250 VAN 4WD, TRANSIT T350 VAN 2WD, TRANSIT T350 VAN 4WD, TRANSIT T350 WAGON 2WD, TRANSIT T350 WAGON 4WD"]
[2021,"FOMOCO","MFMXD06.26BC","MFMXR0250NHJ","Ford","F350 4x4","LFE1-6.2-571",0,6.2,8742,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061481","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.037000000000000005,0.04,"0.20",0.003,"Ford: F250 PICKUP 2WD FFV, F250 PICKUP 4WD FFV, F350 PICKUP 2WD FFV, F350 PICKUP 4WD FFV"]
[2021,"FOMOCO","MFMXD06.27BC","MFMXR0250NHJ","Ford","F350 4x4","LFE1-6.2-571",0,6.2,8742,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061483","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.23070000000000002,0.231,"0.600",0,"Ford: F350 PICKUP 2WD FFV, F350 PICKUP 4WD FFV"]
[2021,"FOMOCO","MFMXT01.52X1","MFMXR0125GDF","Ford","Escape","313W540",0,1.5,3464,4760,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058649","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",3.8E-3,0.004,"0.020",0,"Ford: BRONCO SPORT 4WD, ESCAPE AWD"]
[2021,"FOMOCO","MFMXT02.02MI","MFMXR0130NDF","Ford","Transit Connect FWD","GHC1-2.5-C-753",1,2.5,3968,5280,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HFMX10039896","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1834,0.183,"000.400",0,"Ford: TRANSIT CONNECT VAN FFV, TRANSIT CONNECT WAGON LWB FFV"]
[2021,"FOMOCO","MFMXT02.33MC","MFMXR0135NDG","Ford","Ranger - Chassis Cab","KFG1-2.3-H-367",0,2.3000000000000003,4527,6050,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KFMX10055550","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.010700000000000001,0.011000000000000001,"0.020",0,"Ford: RANGER TREMOR 4WD"]
[2021,"FOMOCO","MFMXT02.53CE","MFMXR0135LLN","Ford","Escape PHEV","LTF1-2.5-010",0,2.5,3884,4860,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","LFMX10063694","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2879,0.29100000000000004,"0.400",3.4000000000000002E-3,"Lincoln: CORSAIR AWD PHEV"]
[2021,"FOMOCO","MFMXT02.72V6","MFMXR0140NDG","Ford","Bronco","MG11-2.7-J-201",0,2.7,5288,6180,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","MFMX10068565","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0097,0.01,"0.020",0,"Ford: BRONCO 4WD, BRONCO BADLANDS 4WD, BRONCO SASQUATCH 4WD"]
[2021,"FOMOCO","MFMXT03.33U3","MFMXR0170NDF","Ford","Explorer","LTW1-3.3-L-477",0,3.3000000000000003,4595,5830,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX91004245","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17170000000000002,0.17200000000000001,"000.400",0,"Ford: EXPLORER FFV AWD"]
[2021,"FOMOCO","MFMXT03.54HF","MFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049674","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Ford: EXPEDITION MAX 2WD, EXPEDITION MAX 4WD  Lincoln: NAVIGATOR L 2WD, NAVIGATOR L 4WD"]
[2021,"FOMOCO","MFMXT03.54JM","MFMXR0260NDG","Ford","F-150 4X4 SUPER CREW CAB","JKC00022",0,2.7,4925,6600,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KFMX10057896","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",4.8000000000000004E-3,0.005,"0.020",0,"Ford: F150 PICKUP TREMOR 4WD, F150 RAPTOR 4WD"]
[2021,"GM","MGMXD04.3392","MGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064691","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2021,"GM","MGMXD06.6394","MGMXF02176BB","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","43GGME1976",0,4.3,7670,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","MGMX10064690","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.38620000000000004,0.386,"0.600",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, SILVERADO 2500 HD 2WD CAB CHAS, SILVERADO 2500 HD 4WD CAB CHAS  GMC: G3500 SAVANA 2WD CUTAWAY CH, SIERRA 2500 HD 2WD CAB CHAS, SIERRA 2500 HD 4WD CAB CHAS"]
[2021,"GM","MGMXT02.0500","MGMXR015740B","GMC","ACADIA AWD","20TLNN5933",0,2,4283,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","LGMX10061439","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.024,0.02,"0.20",0,"Cadillac: XT5 AWD, XT5 FWD, XT6 AWD, XT6 FWD  Chevrolet: BLAZER AWD, BLAZER FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2021,"GM","MGMXT02.5200","MGMXR013835A","GMC","CANYON 4WD","25SPHN1023",0,2.5,4194,5600,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10051247","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.006,0.006,"0.020",0,"Chevrolet: COLORADO 2WD, COLORADO 4WD  GMC: CANYON 2WD, CANYON 4WD"]
[2021,"GM","MGMXT04.3186","MGMXR017350D","GMC","K10 SIERRA 4WD","27KPKN1422",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053403","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.02,0.02,"0.20",0,"Chevrolet: SILVERADO 2WD, SILVERADO 2WD CAB CHASSIS, SILVERADO 4WD, SILVERADO 4WD CAB CHASSIS, SILVERADO 4WD TRAILBOSS  GMC: SIERRA 2WD, SIERRA 2WD CAB CHASSIS, SIERRA 4WD, SIERRA 4WD CAB CHASSIS"]
[2021,"GM","MGMXT06.2375","MGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055638","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.314,0.314,"0.525",0,"Cadillac: ESCALADE 2WD, ESCALADE 4WD  Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD  GMC: YUKON XL 2WD, YUKON XL 4WD"]
[2021,"GM","MGMXV01.4001","MGMXR011230A","BUICK","ENCORE FWD","143SV986DA",0,1.4000000000000001,3195,null,3500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","MGMX10065640","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2272,0.227,"0.300",0,"Buick: ENCORE AWD, ENCORE FWD  Chevrolet: TRAX AWD, TRAX FWD"]
[2021,"GM","MGMXV03.6165","MGMXR013030B","CADILLAC","CTS AWD","206GAE4665",0,2,3947,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JGMX10046504","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: CAMARO"]
[2021,"GM","MGMXV06.2091","MGMXR01383CC","CHEVROLET","CORVETTE","621LYV2252",0,6.2,3715,null,4000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LGMX10062252","MFR","65","Evap Canister Bleed Test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0071,0.007,"0.020",0,"Chevrolet: CORVETTE"]
[2021,"Honda","MHNXT02.09VC","MHNXR01491SA","ACURA","RDX AWD A-SPEC","EKYF4A",0,2,4087,5027,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KHNX10052118","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0099,0.01,"0.020",0,"Acura: RDX AWD A-SPEC, RDX FWD A-SPEC"]
[2021,"Honda","MHNXV01.53EB","MHNXR0150VSB","ACURA","RDX AWD A-SPEC","EKYF4A",0,2,4087,5027,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KHNX10052118","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0099,0.01,"0.020",0,"Honda: ACCORD, ACCORD SPORT/TOURING"]
[2021,"Honda","MHNXV02.0BEB","MHNXR0122VSA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044204","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.013000000000000001,0.01,"0.20",0,"Honda: ACCORD, ACCORD SPORT/TOURING"]
[2021,"Hyundai","MHYXT02.5MP5","MHYXR0144MPG","Kia","Sorento","MQ4U1H5GA042A",0,2.5,3935,5467,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10065283","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.20",0.003,"HYUNDAI MOTOR COMPANY: Santa Fe AWD, Santa Fe FWD"]
[2021,"Hyundai","MHYXT02.5TP5","MHYXR0142TTG","Genesis","GV80","JX-U1L5TA205A",0,3.5,5004,6108,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MHYX10062901","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"GENESIS: GV80 AWD, GV80 RWD"]
[2021,"Hyundai","MHYXV01.6BC5","MHYXR0110BCE","HYUNDAI","Accent","RB1R6GU05A1",0,1.6,2522,3549,2875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CHYX10012076","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.022000000000000002,0.02,"0.05",0,"HYUNDAI MOTOR COMPANY: Veloster"]
[2021,"Hyundai","MHYXV01.6KC5","MHYXR0127KCE","Hyundai","Tucson","LM4N0AU13B2",0,2,3373,4608,3750,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","EHYX10025726","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.016,0.02,"0.05",0,"HYUNDAI MOTOR COMPANY: Kona AWD, Kona FWD"]
[2021,"Hyundai","MHYXV01.6P2T","MHYXR0110P2G","HYUNDAI","IONIQ PHEV","AE8G6WU05AC",0,1.6,3353,4343,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"Y","JHYX10046722","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"HYUNDAI MOTOR COMPANY: Ioniq Plug-in Hybrid"]
[2021,"Hyundai","MHYXV02.0CE3","MHYXR0130CEG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038647","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0056,0.006,"0.020",0,"HYUNDAI MOTOR COMPANY: Elantra"]
[2021,"Hyundai","MHYXV02.0LF5","MHYXR0133LFG","HYUNDAI","Tucson","TL6N0HU03AC",0,2,3489,4740,3750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GHYX10034918","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1709,0.171,"0.300",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2021,"Hyundai","MHYXV02.4LH5","MHYXR0133LHG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10038257","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0112,0.011000000000000001,"0.020",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2021,"Hyundai","MHYXV03.3JK6","MHYXR0140JKG","Genesis","G90","HI-U0T0GA082A",0,5,4960,5864,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LHYX10056908","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",5.8000000000000005E-3,0.006,"0.020",0,"GENESIS: G90 AWD, G90 RWD"]
[2021,"Jaguar Land Rover L","MJLXJ03.0FSC","MJLXR0140P1Z","Land Rover","Range Rover Evoque","3EVPP037",0,2,3995,5181,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","EJLX10028181","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2268,0.227,"0.400",0,"Jaguar: F-PACE P340 MHEV, F-PACE P400 MHEV  Land Rover: Range Rover Velar P340 MHEV, Range Rover Velar P400 MHEV"]
[2021,"Karma Automotive","MKALV01.5K12","MKALR0080K12","Karma","Revero GT","PV2012",4,1.5,5035,5925,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,1,"N","N",null,null,"Y","LKAL10061223","MFR","44","Fed. refuel (orvr) (Heat to load)","47","CARB LEV3 E10 Premium Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.04,0,"0.2",6.29E-4,"Karma Automotive LLC: GS-6 (21-inch wheels), GS-6 (22-inch wheels), Revero GT (21-inch wheels), Revero GT (22-inch wheels)"]
[2021,"Kia","MKMXT02.0NE5","MKMXR0122NEG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038647","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0056,0.006,"0.020",0,"KIA MOTORS CORPORATION: Seltos AWD, Seltos FWD"]
[2021,"Kia","MKMXT02.4HH5","MKMXR0133HHG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10038257","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0112,0.011000000000000001,"0.020",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FWD"]
[2021,"Kia","MKMXV01.6AB6","MKMXR0120ABG","KIA","Rio","SC9R6GU11AC",0,1.6,2727,3616,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LKMX10055987","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"KIA MOTORS CORPORATION: Rio"]
[2021,"Kia","MKMXV01.6DC5","MKMXR0131DCG","Kia","K5","DL3U1G6TA007F",0,1.6,3115,4354,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","MKMX10062908","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.020",0,"KIA MOTORS CORPORATION: K5, K5 AWD"]
[2021,"Kia","MKMXV02.0BE3","MKMXR0114BEG","HYUNDAI","VELOSTER","JS9N0GU01AC",0,2,2844,3748,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","KHYX10051001","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.6000000000000003E-3,0.004,"0.020",0,"KIA MOTORS CORPORATION: Soul, Soul Eco dynamics"]
[2021,"Kia","MKMXV02.5DP5","MKMXR0133DPG","Hyundai","Sonata","DN8U0H5GA023F",0,2.5,3120,4354,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LHYX10059891","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.02",0,"KIA MOTORS CORPORATION: K5"]
[2021,"Maserati","MMAXJ03.0DFI","MMAXR0110161","MASERATI","QUATTROPORTE GTS","070989",1,3.8000000000000003,4495,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","HMAX10042289","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",2E-3,0.01,"0.20",0.01,"MASERATI: GHIBLI, GHIBLI S, GHIBLI S Q4, LEVANTE, LEVANTE S, QUATTROPORTE S, QUATTROPORTE S Q4"]
[2021,"MAZDA","MTKXV02.5CDA","MTKXR0107GBK","MAZDA","CX-3","0ECPEUG1-034",0,2,2994,3990,3250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LTKX10059557","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL-EQUIV",0.35900000000000004,0.37,"0.50",0.012,"MAZDA: CX-3 2WD, CX-3 4WD"]
[2021,"Mercedes-Benz","MMBXD02.0HD1","MMBXR0170LNB","Mercedes-Benz","Metris (Passenger Van)","L447E20DETC-Z6027",0,1.991,4992,6724,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","GMBX10037689","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4364,0.436,"0.475",0,"Mercedes-Benz: Freightliner Sprinter 1500, Freightliner Sprinter 2500, Sprinter 1500, Sprinter 2500"]
[2021,"Mercedes-Benz","MMBXJ03.0U2A","MMBXR0155LNC","Mercedes-Benz","C 300 4MATIC","Z5023",0,1.991,3715,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10037449","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2624,0.262,"0.275",0,"Mercedes-Benz: AMG C 43 4MATIC, AMG C 43 4MATIC (convertible), AMG C 43 4MATIC (coupe), AMG C 43 4MATIC (station wagon), AMG GLC 43 4MATIC, AMG GLC 43 4MATIC (coupe)"]
[2021,"Mercedes-Benz","MMBXT04.0HY3","MMBXR0170LNC","Mercedes-Benz","GLE 550 4MATIC","W166E46DETC-Z6018",0,4.664000000000001,5200,6500,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","HMBX10039926","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4544,0.454,"0.475",0,"Mercedes-Benz: AMG GLS 63 4MATIC+, GLS 600 4MATIC Maybach"]
[2021,"Mercedes-Benz","MMBXV02.0U3B","MMBXR0095LNB","Mercedes-Benz","AMG CLA 45 4MATIC+","C118E20DETC-Z2019",2,1.991,3719,4729,4000,"4","4-Wheel Drive","AM","Automated Manual",null,8,"Y","N",null,null,"N","LMBX10065608","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Mercedes-Benz: AMG CLA 45 4MATIC, AMG GLA 45 4MATIC"]
[2021,"Mercedes-Benz","MMBXV04.0U3A","MMBXR0170LNS","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10035378","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2048,0.24,"0.275",0.035,"Mercedes-Benz: AMG GT Black Series"]
[2021,"Mitsubishi Motors Co","MMTXT02.4H3M","MMTXR0148A2L","MITSUBISHI","OUTLANDER PHEV","EB18-RH43",0,1.998,4292,5225,4750,"F","2-Wheel Drive, Front","A","Automatic",null,1,"Y","N",null,null,"Y","JMTX10047881","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0177,0.018000000000000002,"0.200",0,"Mitsubishi Motors Corporation: Outlander PHEV"]
[2021,"Nissan","MNSXT02.0AVA","MNSXR0140PEA","INFINITI","QX55 AWD SENSORY","CPE692",1,2,4134,5062,4500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","MNSX10063359","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.07,0.09,"0.20",0.019,"INFINITI: QX50, QX50 AWD, QX55 AWD"]
[2021,"Nissan","MNSXT05.6N9B","MNSXR0201PFA","INFINITI","QX80 4WD SENSORY","TWE530",0,5.6000000000000005,6081,7412,6500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","MNSX10062726","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"INFINITI: QX80 2WD, QX80 4WD  NISSAN: ARMADA 2WD, ARMADA 4WD"]
[2021,"Nissan","MNSXT05.6P9A","MNSXR0201PFA","NISSAN","TITAN 4WD PRO-4X","TVC364",1,5.6000000000000005,5855,7300,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","JNSX10050855","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.08,0.08,"0.20",0,"NISSAN: TITAN 2WD, TITAN 4WD, TITAN 4WD PRO-4X"]
[2021,"Nissan","MNSXV03.5P7C","MNSXR0149PCA","NISSAN","MURANO AWD SL","JJE437",0,3.5,4151,5280,4500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LNSX10061875","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.008,"0.020",0,"NISSAN: MURANO AWD, MURANO FWD"]
[2021,"Pagani S.p.A.","MPGNV06.0ABC","MPGNR0170AA2","Pagani Automobili","Huayra Roadster BC","ZA9H12EAYYSF76002",0,6,3091,3748,3375,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LPGN10065612","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.01,0,"0.2",0.02,"Certification: Pagani Huayra"]
[2021,"Porsche","MPRXT03.0CV6","MPRXR0150REE","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX10054422","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.3559,0.37,"0.450",0.014,"Porsche: Cayenne, Cayenne Coupé, Cayenne S, Cayenne S Coupé"]
[2021,"Porsche","MPRXV04.0S82","MPRXR0170R92","Porsche","911 Carrera S","EC-992S-PDK-20",0,3,3382,4376,3875,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"N","MPRX10065417","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2301,0.23,"0.300",0,"Porsche: 911 Turbo, 911 Turbo Cabriolet, 911 Turbo S, 911 Turbo S Cabriolet"]
[2021,"Subaru","MFJXJ02.5BUY","MFJXR01155AD","SUBARU","IMPREZA 5-Door","HBV-YU15",1,2,3195,4299,3500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N","HFJX10042772","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.005,0.01,"0.20",0.004,"Subaru: IMPREZA 4-Door, IMPREZA 4-Door SPORT, IMPREZA 5-Door, IMPREZA 5-Door SPORT"]
[2021,"Toyota","MTYXJ02.5N4L","MTYXR0130P72","TOYOTA","CAMRY XLE/XSE","18-AV1A",1,2.487,3415,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","JTYX10046336","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.012100000000000001,0.012,"0.020",0,"LEXUS: ES 250 AWD  TOYOTA: AVALON AWD, CAMRY AWD LE/SE, CAMRY AWD XLE/XSE, RAV4, RAV4 AWD, RAV4 AWD LE, RAV4 AWD TRD OFFROAD"]
[2021,"Toyota","MTYXT02.5P34","MTYXR0195J82","TOYOTA","SIENNA AWD","21-AL1H",0,2.487,4825,6170,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","MTYX10065381","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.19690000000000002,0.197,"0.400",0,"TOYOTA: SIENNA, SIENNA AWD"]
[2021,"Toyota","MTYXT05.7K6Y","MTYXR0190P32","TOYOTA","TOYOTA TUNDRA 2WD","05-GSK1",2,3.9560000000000004,4270,5700,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","7TYX10000758","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","150","HC",0.004,0,"0.05",0,"LEXUS: LX 570  TOYOTA: LAND CRUISER WAGON 4WD"]
[2021,"Toyota","MTYXV01.8P35","MTYXR0130J72","TOYOTA","PRIUS PRIME","17-ZW3H",0,1.798,3365,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HTYX10042566","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1353,0.135,"0.300",0,"TOYOTA: PRIUS PRIME"]
[2021,"Toyota","MTYXV02.0P3A","MTYXR0130P72","TOYOTA","CAMRY XLE/XSE","18-AV1A",1,2.487,3415,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","JTYX10046336","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.012100000000000001,0.012,"0.020",0,"TOYOTA: COROLLA, COROLLA APEX, COROLLA HATCHBACK, COROLLA HATCHBACK MANUAL, COROLLA HATCHBACK XSE, COROLLA XSE"]
[2021,"Toyota","MTYXV03.5M5C","MTYXR0180A72","LEXUS","LC 500","18-UZ2A",0,4.969,4280,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N","JTYX10045648","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.007,0.01,"0.05",0,"LEXUS: LS 500, LS 500 AWD"]
[2021,"Volkswagen Group of","MVGAJ02.0A7G","MVGAR0140ACN","AUDI","SQ5","H7NF-SQ5",0,2.995,4398,5732,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVGA10045596","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.016,0.016,"0.020",0,"Audi: Q5, Q5 Sportback"]
[2021,"Volkswagen Group of","MVGAJ02.0V3A","MVGAR0135ACT","VOLKSWAGEN","Tiguan","UTI035",1,1.984,3885,5247,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVGA10048049","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24500000000000002,0.24500000000000002,"0.350",0,"Volkswagen: Tiguan, Tiguan 4Motion"]
[2021,"Volkswagen Group of","MVGAT03.0N7M","MVGAR0150NCM","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX10054422","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3559,0.37,"0.450",0.014039999999999999,"Audi: Q7, Q8"]
[2021,"Volkswagen Group of","MVGAT03.6VAS","MVGAR0135VCS","VOLKSWAGEN","Atlas","VW416070129",0,3.6,4713,5732,5000,"A","All Wheel Drive","A","Automatic",null,8,"Y","N",null,null,"N","JVGA10046317","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015700000000000002,0.016,"0.020",0,"Volkswagen: Atlas, Atlas 4Motion, Atlas Cross Sport, Atlas Cross Sport 4Motion"]
[2021,"Volkswagen Group of","MVGAV02.0VAB","MVGAR0135ACU","VOLKSWAGEN","Arteon","VW483-09-0158",0,1.984,3719,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KVGA10057701","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.081,0.08,"0.20",0,"Volkswagen: Arteon, Arteon 4Motion"]
[2021,"Volkswagen Group of","MVGAV02.9N7S","MVGAR0150NCS","AUDI","A8L","KN7M-D5",0,2.995,4806,null,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KVGA10055600","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.184,0.20900000000000002,"0.300",0.025,"Audi: S6, S7"]
[2021,"Volkswagen Group of","MVGAV05.2NDE","MVGAR0155NAL","AUDI","R8","LNBE-R8B",2,5.204000000000001,3968,null,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LVGA10058208","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.341,0.35000000000000003,"0.65",0.013000000000000001,"Lamborghini: Huracan, Huracan 2WD, Huracan STO, Huracan Spyder, Huracan Spyder 2WD"]
[2021,"Volvo","MVVXJ02.0S30","MVVXR0142E51","Volvo","XC60 T6 AWD","201812",0,1.969,4268,5475,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVVX10047698","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0132,0.013000000000000001,"0.020",0,"Volvo Cars of North America, LLC: S60 AWD, S90 AWD, V60 AWD, V90 AWD"]
[2021,"Volvo","MVVXJ02.0U70","MVVXR0142E51","Volvo","XC60 T6 AWD","201812",0,1.969,4268,5475,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVVX10047777","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.008,0.008,"0.200",0,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD, V60 FWD, V90 FWD, XC60 FWD"]
[2020,"BMW","LBMXJ02.0B4X","LBMXR0130F3X","BMW","330i","5D42601",0,2,3541,4530,3875,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10042276","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","4","HC-TOTAL-EQUIV",0.0032,0.003,"0.020",0,"BMW: 228i XDRIVE GRAN COUPE, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, 330i xDrive Gran Turismo, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe"]
[2020,"BMW","LBMXJ03.0B07","LBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044891","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","4","HC-TOTAL-EQUIV",0.0035,0.004,"0.020",0,"BMW: 840i Convertible, 840i Coupe, 840i Gran Coupe, 840i xDrive Convertible, 840i xDrive Coupe, 840i xDrive Gran Coupe  TOYOTA: Supra 3.0"]
[2020,"BMW","LBMXJ03.0B07","LBMXR0180G05","BMW","X5 xDrive50i","LB15156",0,4.4,5170,6460,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KBMX10053878","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.01,0.01,"0.05",0,"BMW: X5 sDrive40i, X5 xDrive40i, X6 sDrive40i, X6 xDrive40i, X7 xDrive40i"]
[2020,"BMW","LBMXT03.0S58","LBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044990","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0.005,0,"0.02",0,"BMW: X3 M, X3 M Competition, X4 M, X4 M Competition"]
[2020,"BMW","LBMXV01.5B36","LBMXR0130F45","Mini","Mini Cooper Countryman","3B62508",0,1.5,3360,4376,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HBMX91003343","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2043,0.20400000000000001,"0.275",0,"Mini: COOPER CLUBMAN, COOPER CLUBMAN ALL4, COOPER COUNTRYMAN, COOPER COUNTRYMAN ALL4"]
[2020,"BMW","LBMXV02.0B46","LBMXR0100F5X","Mini","MINI COOPER HARDTOP 2 DOOR","T739201",5,1.5,2690,3565,3000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HBMX10040821","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.036000000000000004,0.04,"0.20",0,"Mini: COOPER S CONVERTIBLE, COOPER S HARDTOP 2 DOOR, COOPER S HARDTOP 4 DOOR, JOHN COOPER WORKS CONVERTIBLE, JOHN COOPER WORKS HARDTOP"]
[2020,"FCA US LLC","LCRXD03.65V2","LCRXR0180TP1","RAM","Promaster 1500","L0VF12863",0,3.6,6500,8550,6500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LCRX10060538","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1326,0.138,"0.550",0.0057,"RAM: Promaster 1500, Promaster 2500, Promaster 3500"]
[2020,"FCA US LLC","LCRXD06.45V4","LCRXF0205TC0","Dodge","RAM 3500 CAB CHAS 2WD","K7DC88916",0,5.7,10000,12500,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","9CRX01070370","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.7000000000000001,0.7000000000000001,"1.4",0,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2020,"FCA US LLC","LCRXD06.45W3","LCRXR0353TC1","RAM","2500 Cab Chassis 4X4","L0DJ79243",0,6.4,8925,10000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10066249","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.7250000000000001,0.72,"1.25",0,"RAM: 3500 4X2, 3500 4X4"]
[2020,"FCA US LLC","LCRXJ02.05P2","LCRXR0108PP0","Alfa Romeo","650","L7GUF8294",1,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10048785","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"ALFA ROMEO: Giulia, Giulia AWD"]
[2020,"FCA US LLC","LCRXT02.05P3","LCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050400","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Jeep: Wrangler Unlimited 4x4"]
[2020,"FCA US LLC","LCRXT02.45P1","LCRXR0110PP2","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043880","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2414,0.25,"0.300",0.009000000000000001,"Jeep: Renegade 4x2, Renegade 4x4"]
[2020,"FCA US LLC","LCRXT03.25P0","LCRXR0118PP0","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043878","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2566,0.262,"0.375",0.0057,"Jeep: Cherokee 4X4, Cherokee 4x4 Active Drive II, Cherokee FWD, Cherokee Trailhawk 4X4"]
[2020,"FCA US LLC","LCRXT03.65P6","LCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045054","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1829,0.192,"0.450",0.009000000000000001,"Chrysler: Pacifica Hybrid"]
[2020,"FCA US LLC","LCRXT05.75P1","LCRXR0183RP1","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049483","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.03,0.03,"0.20",0,"RAM: 1500 4X2, 1500 4X4"]
[2020,"FCA US LLC","LCRXT05.75P2","LCRXR0183RP1","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049482","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 Classic 4X2, 1500 Classic 4X4"]
[2020,"FCA US LLC","LCRXT06.25P1","LCRXR0180RK0","Jeep","Grand Cherokee 4wd","K1WKJ8647",0,3.6,4716,6500,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BCRX10008679","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Jeep: Grand Cherokee Trackhawk 4x4"]
[2020,"FCA US LLC","LCRXV01.45P0","LCRXR0107PK1","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017735","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.41200000000000003,0.41000000000000003,"0.50",0,"FIAT: 124 Spider"]
[2020,"FCA US LLC","LCRXV05.75P5","LCRXR0141PK0","Dodge","Charger SRT","L0LDD6582",1,6.4,4415,5450,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LCRX10062607","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL-EQUIV",0.449,0.46,"0.50",0.01,"Dodge: Challenger, Charger"]
[2020,"FCA US LLC","LCRXV06.45P0","LCRXR0141PK0","Chrysler","300 AWD","L5LXF1269",3,3.6,4324,5350,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","HCRX10044798","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.444,0.45,"0.50",0.01,"Dodge: Challenger, Challenger Widebody, Charger, Charger Widebody"]
[2020,"FOMOCO","LFMXD03.56BG","LFMXR0185NDJ","Ford","T150 Transit Van MDPV","LTH1-3.5-J-429",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10060896","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.016,0.02,"0.05",0,"Ford: TRANSIT T150 VAN 2WD FFV, TRANSIT T150 VAN 4WD FFV, TRANSIT T250 VAN 2WD FFV, TRANSIT T250 VAN 4WD FFV, TRANSIT T350 VAN 2WD FFV, TRANSIT T350 VAN 4WD FFV, TRANSIT T350 WAGON 2WD FFV, TRANSIT T350 WAGON 4WD FFV"]
[2020,"FOMOCO","LFMXD06.26BC","LFMXF0360NHJ","Ford","F350 4x4","LFE1-6.2-J-578",0,6.2,9000,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061062","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Ford: F250 2WD BED DELETE FFV, F250 4WD BED DELETE FFV, F350 2WD BED DELETE FFV, F350 4WD BED DELETE FFV"]
[2020,"FOMOCO","LFMXD06.27BC","LFMXF0250NDJ","Ford","F350 4x4","LFE1-6.2-571",0,6.2,8742,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061480","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3521,0.35200000000000004,"0.600",0,"Ford: F350 2WD BED DELETE FFV, F350 4WD BED DELETE FFV"]
[2020,"FOMOCO","LFMXD07.373K","LFMXR0360NHJ","Ford","F350 4x4","LFE1-6.2-J-578",0,6.2,9000,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LFMX10061611","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0131,0.013000000000000001,"0.030",0,"Ford: F350 2WD, F350 4WD"]
[2020,"FOMOCO","LFMXT01.01B7","LFMXR0090GDE","Ford","EcoSport","JBW1-2.0-J-073",1,2,3389,4253,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JFMX10049006","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1675,0.168,"0.300",0,"Ford: ECOSPORT FWD"]
[2020,"FOMOCO","LFMXT02.02Y1","LFMXR0125GDF","Ford","Escape","LTC1-1.5-H-527",0,1.5,3514,4760,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","LFMX10058645","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"000.05",2E-3,"Ford: ESCAPE AWD, ESCAPE FWD  Lincoln: CORSAIR AWD, CORSAIR FWD"]
[2020,"FOMOCO","LFMXT03.03P1","LFMXR0165LDG","Ford","Explorer Police FHEV","LTW1-3.3-L-471",0,3.3000000000000003,5095,6840,5500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","LFMX10059621","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",2E-3,0,"0.20",2E-3,"Lincoln: AVIATOR AWD PHEV"]
[2020,"FOMOCO","LFMXT03.33DU","LFMXR0260NDG","Ford","F150-Super Cab gas 4x4","JFC1-3.3-J-028",3,3.3000000000000003,4687,6500,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JFMX10049037","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.007,0.01,"0.20",0.003,"Ford: F150 2WD FFV BASE PAYLOAD LT, F150 4WD FFV BASE PAYLOAD LT, F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2020,"FOMOCO","LFMXT05.03DP","LFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049673","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2212,0.221,"0.500",0,"Ford: F150 2WD FFV BASE PAYLOAD LT, F150 4WD FFV BASE PAYLOAD LT, F150 5.0L 2WD FFV GVWR>7599 LBS, F150 5.0L 4WD FFV GVWR>7599 LBS, F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2020,"FOMOCO","LFMXV02.0VZ7","LFMXR0145HCE","Lincoln","MKZ (HEV)","HC91-2.0-J-815",0,2,3919,4910,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HFMX91003073","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.15080000000000002,0.151,"0.300",0,"Ford: FUSION POLICE RESPONDER HEV"]
[2020,"FOMOCO","LFMXV03.0VLG","LFMXR0135NDE","Lincoln","Continental","HPL1-3.7-J-838",0,3.7,4517,5560,4750,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","HFMX10048125","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.004,0.004,"0.020",0,"Lincoln: CONTINENTAL AWD, CONTINENTAL COACH"]
[2020,"GM","LGMXD06.0395","LGMXR0223841","CHEVROLET","G3500 EXPRESS 2WD PASS","43GCJNT213",2,4.3,6249,9600,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10051629","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.543,0.54,"1.00",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G2500 EXPRESS 2WD PASS INCOM, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G2500 SAVANA 2WD PASS INCOM, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2020,"GM","LGMXD06.6394","LGMXR021260A","CHEVROLET","SILVERADO 2WD","66CRLN1016",0,6.6000000000000005,6761,10350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","LGMX10057418","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2020,"GM","LGMXT02.0400","LGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035628","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Cadillac: XT4 AWD, XT4 FWD"]
[2020,"GM","LGMXT02.5200","LGMXR012637A","BUICK","ENVISION AWD","204GXN5322",0,2,4128,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10035629","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.026000000000000002,0.03,"0.20",0,"Buick: ENVISION AWD, ENVISION FWD"]
[2020,"GM","LGMXT02.7100","LGMXR022450C","CHEVROLET","K10 SILVERADO 4WD","27KPKN1432",0,2.7,4752,6900,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10055693","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.012,0.012,"0.020",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD"]
[2020,"GM","LGMXT05.3385","LGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053899","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1981,0.198,"0.500",0,"Chevrolet: SILVERADO 2WD, SILVERADO 4WD  GMC: SIERRA 2WD, SIERRA 4WD"]
[2020,"GM","LGMXT06.2375","LGMXR017350D","GMC","K10 SIERRA 4WD","27CPKN1039",0,2.7,5092,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","KGMX10053900","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: SILVERADO 4WD, SILVERADO 4WD TRAILBOSS  GMC: SIERRA 4WD, SIERRA 4WD AT4"]
[2020,"GM","LGMXV02.0031","LGMXR011030C","CHEVROLET","MALIBU","151GZV4303",1,1.5,3334,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","KGMX10054118","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.067,0.07,"0.20",0,"Buick: REGAL, REGAL AWD, REGAL TOUR X AWD  Chevrolet: MALIBU"]
[2020,"GM","LGMXV03.0043","LGMXR01103AA","CADILLAC","CT5 AWD","206LDN4683",0,2,3894,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","LGMX10060941","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2514,0.251,"0.300",0,"Cadillac: CT5, CT5 AWD, CT5 V, CT5 V AWD"]
[2020,"GM","LGMXV04.2088","LGMXR0112835","CADILLAC","CT6","206KKN4481",2,2,3826,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KGMX10057964","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.232,0.23,"0.50",0,"Cadillac: CT6 AWD"]
[2020,"Honda","LHNXT02.08VC","LHNXR01491SA","ACURA","RDX AWD A-SPEC","EKYF4A",0,2,4087,5027,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KHNX10052118","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0099,0.01,"0.020",0,"Acura: RDX AWD, RDX FWD"]
[2020,"Honda","LHNXT03.5J4C","LHNXR01502SA","HONDA","ODYSSEY FWD","EHMR3A",0,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10046194","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.011600000000000001,0.012,"0.020",null,"Honda: ODYSSEY FWD"]
[2020,"Honda","LHNXV01.5TBC","LHNXR0113VSB","HONDA","CIVIC 4DR SEDAN 1.5L","EGAA4C",0,1.5,2908,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10037943","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Honda: CIVIC 2DR, CIVIC 4Dr"]
[2020,"Honda","LHNXV02.07DM","LHNXR0127VSA","HONDA","CR-V 1.5L TC","EHPA2C",0,1.5,3562,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX91003344","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.15480000000000002,0.155,"0.300",0,"Honda: ACCORD"]
[2020,"Honda","LHNXV02.0CL3","LHNXR0113VSA","HONDA","CIVIC 4DR SEDAN 2.0L","EGBB4C",0,2,2808,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10038051","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.20170000000000002,0.202,"0.300",0,"Honda: CIVIC 2DR, CIVIC 4Dr"]
[2020,"Honda","LHNXV03.5PBM","LHNXR0150VSA","HONDA","ODYSSEY FWD","EHMR3A",0,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10046192","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.11,0.1,"0.3",null,"Honda: PILOT AWD, PILOT FWD"]
[2020,"Honda","LHNXV03.5PBM","LHNXR0151VFA","ACURA","RLX","EJ9P2A",0,3.5,3977,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10048469","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL-EQUIV",0,0,"0.05",0,"Acura: MDX AWD, MDX AWD A-spec, MDX FWD"]
[2020,"Hyundai","LHYXV01.6AB6","LHYXR0120ABG","KIA","Rio","SC9R6GU11AC",0,1.6,2727,3616,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LKMX10055985","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",2.8E-3,0.003,"0.020",0,"HYUNDAI MOTOR COMPANY: Accent"]
[2020,"Hyundai","LHYXV02.0BE5","LHYXR0115BEG","HYUNDAI","VELOSTER","JS9N0GU01AC",0,2,2844,3748,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","KHYX10051001","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",3.6000000000000003E-3,0.004,"0.020",0,"HYUNDAI MOTOR COMPANY: Veloster"]
[2020,"Hyundai","LHYXV02.0CE3","LHYXR0130CEG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038647","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0056,0.006,"0.020",0,"HYUNDAI MOTOR COMPANY: Elantra, Elantra SE"]
[2020,"Hyundai","LHYXV02.0LF5","LHYXR0133LFG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10047288","MFR","68","Leak Test - Port Near Fuel Pipe","58","Tier 3 E10 Regular Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.020",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2020,"Hyundai","LHYXV02.4LH5","LHYXR0133LHG","HYUNDAI","Tucson","TL6N0HU03AC",0,2,3489,4740,3750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GHYX10034919","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2484,0.248,"0.300",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2020,"Hyundai","LHYXV02.4MH5","LHYXR0135MHG","KIA","SEDONA","YP9L3AU07AC",0,3.3000000000000003,4740,6085,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KKMX10050561","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2237,0.224,"0.300",0,"HYUNDAI MOTOR COMPANY: Santa Fe AWD, Santa Fe FWD"]
[2020,"Hyundai","LHYXV03.8HL5","LHYXR0140HME","HYUNDAI","Genesis","DH5T0GU11A2",0,5,4724,5710,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FHYX10028453","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.29,0.29,"0.50",0,"GENESIS: G80 AWD, G80 RWD"]
[2020,"Jaguar Land Rover L","LJLXJ05.0FSM","LJLXR0140P1Z","Land Rover","Range Rover Evoque","3EVPP037",0,2,3995,5181,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","EJLX10028181","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2268,0.227,"0.400",0,"Jaguar: F-PACE  Land Rover: Range Rover Velar"]
[2020,"Kia","LKMXT02.0HG5","LKMXR0133HGG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10038282","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.004,0,"0.20",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FWD"]
[2020,"Kia","LKMXT02.4HH5","LKMXR0133HHG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10038257","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0112,0.011000000000000001,"0.020",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FWD"]
[2020,"Kia","LKMXV01.6AB6","LKMXR0110ABG","KIA","Rio","SC9R6GU11AC",0,1.6,2727,3616,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","LKMX10055984","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.01,0.01,"0.20",2E-3,"KIA MOTORS CORPORATION: Rio"]
[2020,"Kia","LKMXV02.0BE3","LKMXR0110BEG","HYUNDAI","VELOSTER","JS9N0GU01AC",0,2,2844,3748,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","KHYX10051001","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",3.6000000000000003E-3,0.004,"0.020",0,"KIA MOTORS CORPORATION: Soul, Soul Eco dynamics"]
[2020,"Kia","LKMXV02.0D13","LKMXR0143D1E","HYUNDAI","SONATA HYBRID","HLF6NAUP13A",0,2,3649,4630,4000,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"Y","GHYX10033968","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.29500000000000004,0.3,"0.50",0,"KIA MOTORS CORPORATION: Optima Hybrid"]
[2020,"Kia","LKMXV02.4DH5","LKMXR0140DHG","HYUNDAI","Sonata","LF5F0TU51A1",0,2,3505,4630,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FHYX10040736","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","3Z","California LEV-III Zero Evap (Option 1)","150","LEAK-DIA",0,0,"0.02",0,"KIA MOTORS CORPORATION: Optima, Optima FE"]
[2020,"Kia","LKMXV03.3FJ6","LKMXR0146FJE","Kia","Cadenza","YG7L3AU13AC",0,3.3000000000000003,3787,4784,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HKMX10041818","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.198,0.2,"0.50",0,"KIA MOTORS CORPORATION: Cadenza"]
[2020,"Koenigsegg","LKGGV05.0RH5","LKGGR0130GBK","Koenigsegg","CCX","HS007031",0,4.7,3075,3800,3375,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N","8KGG10029092","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.327,0.34,"0.50",0.013000000000000001,"Koenigsegg Automotive AG: REGERA"]
[2020,"MAZDA","LTKXV02.0FFA","LTKXR0107GBK","MAZDA","CX-3","0ECPEUG1-034",0,2,2994,3990,3250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","LTKX10059556","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL-EQUIV",0,0,"0.05",0,"MAZDA: CX-3 2WD, CX-3 4WD"]
[2020,"McLaren Automotive ","LMLNV04.0M14","LMLNR0164M14","McLaren","720S Coupe","SBM14AAA8HW990014",0,3.994,3139,3793,3625,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"N","N",null,null,"N","JMLN10047190","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.049,0.05,"0.05",0,"McLaren: 720S Coupe, 720S Spider, Sabre"]
[2020,"Mercedes-Benz","LMBXJ04.0U2A","LMBXR0170LNS","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10035377","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Mercedes-Benz: AMG S 63 4MATIC+, AMG S 63 4MATIC+ (convertible), AMG S 63 4MATIC+ (coupe), S 560, S 560 (convertible), S 560 4MATIC, S 560 4MATIC (W), S 560 4MATIC (coupe), S 560 4MATIC Maybach"]
[2020,"Mercedes-Benz","LMBXT03.0HY1","LMBXR0170LNF","Mercedes-Benz","GLE 550 4MATIC","W166E46DETC-Z6018",0,4.664000000000001,5200,6500,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","HMBX10039926","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.4544,0.454,"0.475",0,"Mercedes-Benz: GLE 450 4MATIC"]
[2020,"Mercedes-Benz","LMBXT04.0HY1","LMBXR0170LNF","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10048076","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.017400000000000002,0.017,"0.020",0,"Mercedes-Benz: GLE 580 4MATIC, GLS 580 4MATIC"]
[2020,"Mercedes-Benz","LMBXV03.0HY2","LMBXR0155LNA","Mercedes-Benz","AMG C 63 4MATIC","W205E40DETC-Z5020",0,3.982,3928,4883,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10035307","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.3509,0.35100000000000003,"0.375",0,"Mercedes-Benz: AMG CLS 53 4MATIC+, AMG E 53 4MATIC+, AMG E 53 4MATIC+ (Convertible), AMG E 53 4MATIC+ (Coupe), AMG E 53 4MATIC+ (Station Wagon)"]
[2020,"Mercedes-Benz","LMBXV05.5U2A","LMBXR0155LNS","Mercedes-Benz","SL 550","R231E46DETC-Z7029",2,4.664000000000001,4050,4795,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N","LMBX10061406","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Mercedes-Benz: SL 550"]
[2020,"Mitsubishi Motors Co","LMTXT02.4G5Z","LMTXR0135A2E","MITSUBISHI","OUTLANDER 2WD","EB18-RB5A",5,2.36,3345,4795,3625,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,6,"Y","N",null,null,"N","JMTX10046918","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.222,0.258,"0.3000",0.036000000000000004,"Mitsubishi Motors Corporation: OUTLANDER 4WD"]
[2020,"Nissan","LNSXD04.0V6B","LNSXF0174PBA","NISSAN","NISSAN NV3500 M S/R","TYB016",0,5.6000000000000005,6187,9900,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","CNSX10011388","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","HD-3D","Federal Heavy-Duty 3-Day Evap (1.4 grams)","120","HC-TOTAL",0.49,0.5,"1.4",0,"NISSAN: NV1500 CARGO VAN, NV2500 CARGO VAN, NV3500 PASSENGER VAN"]
[2020,"Nissan","LNSXT02.5R5A","LNSXR0114PEA","NISSAN","ROGUE AWD","BTEL15",0,2.5,3653,4720,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","JNSX10048366","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2748,0.275,"0.400",0,"NISSAN: ROGUE AWD, ROGUE FWD"]
[2020,"Nissan","LNSXV02.0PMA","LNSXR0114PCB","NISSAN","ALTIMA SR/PLATINUM","FRB170",0,2.5,3443,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","KNSX10054246","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.010700000000000001,0.011000000000000001,"0.020",0,"NISSAN: Qashqai, Qashqai AWD, Rogue Sport, Rogue Sport AWD"]
[2020,"Nissan","LNSXV02.5RPA","LNSXR0114PCB","NISSAN","ALTIMA SR/PLATINUM","FRB170",0,2.5,3443,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","KNSX91003970","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2364,0.23600000000000002,"0.300",0,"NISSAN: ALTIMA, ALTIMA AWD, ALTIMA AWD SR/PLATINUM, ALTIMA SR/PLATINUM"]
[2020,"Porsche","LPRXT03.0CH6","LPRXR0145REH","Porsche","Cayenne e-Hybrid","ECFE-9YAH-19",0,3,5311,6680,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KPRX10059259","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2026,0.215,"0.500",0.0126,"Porsche: Cayenne e-Hybrid, Cayenne e-Hybrid Coupé"]
[2020,"Porsche","LPRXT04.0CV8","LPRXR0150REE","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX10054422","MFR","34","Federal fuel 3-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.3559,0.37,"0.450",0.014,"Porsche: Cayenne Turbo, Cayenne Turbo Coupé"]
[2020,"Porsche","LPRXV02.5B82","LPRXR0130R82","Porsche","Cayman S","ECFE-982S-PDK-20",0,2.5,3210,3737,3500,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LPRX10064332","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRA","Mfr. Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.006,0.03,"0.20",0.02,"Porsche: Boxster, Boxster S, Boxster T, Cayman, Cayman S, Cayman T"]
[2020,"Roush","LRIIT05.03DP","LRIIR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10049674","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",1E-3,0,".05",0,"Roush Industries, Inc.: F150 Pickup 2WD, F150 Pickup 4WD"]
[2020,"Subaru","LFJXJ02.4CZA","LFJXR01435DA","SUBARU","OUTBACK AWD","LBV-YBA6",0,2.4,3931,5026,4250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N","LFJX10057378","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Subaru: LEGACY, OUTBACK AWD"]
[2020,"Subaru","LFJXT02.0EVC","LFJXR01485JG","SUBARU","CROSSTREK","KBV-CG193",0,2,3766,4901,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","KFJX91003939","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1802,0.18,"0.400",0,"Subaru: CROSSTREK HYBRID AWD"]
[2020,"Toyota","LTYXT03.5M5M","LTYXR0165P82","TOYOTA","SIENNA AWD","17-GL4A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","HTYX10042218","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0046,0.005,"0.020",0,"LEXUS: RX 350, RX 350 AWD, RX 350L, RX 350L AWD  TOYOTA: HIGHLANDER, HIGHLANDER AWD, SIENNA, SIENNA AWD"]
[2020,"Toyota","LTYXT04.6K6W","LTYXR0190P32","TOYOTA","TOYOTA TUNDRA 2WD","05-GSK1",0,3.9560000000000004,4270,5700,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","5TYX01057917","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","150","HC",0.02,0.03,"0.20",0.013000000000000001,"LEXUS: GX 460"]
[2020,"Toyota","LTYXV02.0N4A","LTYXR0130P72","TOYOTA","CAMRY XLE/XSE","18-AV1A",1,2.487,3415,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","JTYX10046255","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.003,0,"0.20",0,"LEXUS: UX 200"]
[2020,"Toyota","LTYXV02.5P33","LTYXR0165J72","TOYOTA","CAMRY HYBRID XLE/SE","18-AV3H",0,2.487,3565,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","JTYX10047585","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1683,0.168,"0.300",0,"LEXUS: ES 300h  TOYOTA: AVALON HYBRID, AVALON HYBRID XLE, CAMRY HYBRID XLE/SE"]
[2020,"Toyota","LTYXV03.5M5A","LTYXR0165P12","LEXUS","IS 300","19-AE2A",2,1.998,3760,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","LTYX10062316","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"LEXUS: GS 350, GS 350 AWD, GS 350 F SPORT, IS 300 AWD, IS 350, IS 350 AWD, RC 300 AWD, RC 350, RC 350 AWD"]
[2020,"Volkswagen Group of","LVGAJ02.0AAC","LVGAR0140ACP","AUDI","A4","HAAC-BAQ",4,1.984,4035,null,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","HVGA10045300","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.24300000000000002,0.273,"0.300",0.03,"Audi: A4 allroad quattro, A4 quattro, A5 Cabriolet quattro, A5 Sportback quattro, A5 quattro"]
[2020,"Volkswagen Group of","LVGAJ03.0NAP","LVGAR0150NCY","AUDI","A8 e-tron","LNAP-A8",0,2.995,5380,5622,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","LVGA10061117","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.028,0.034,"0.200",0.006,"Audi: A8L"]
[2020,"Volkswagen Group of","LVGAT03.0NAQ","LVGAR0155NCV","Porsche","Cayenne e-Hybrid","ECFE-9YAH-19",0,3,5311,6680,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KPRX10059259","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2026,0.216,"0.500",0.013000000000000001,"Bentley: Bentayga"]
[2020,"Volkswagen Group of","LVGAT04.0PAA","LVGAR0155ECR","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX10054428","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.036000000000000004,0.043000000000000003,"0.200",0.007,"Bentley: Bentayga  Lamborghini: Urus"]
[2020,"Volkswagen Group of","LVGAV01.4V7P","LVGAR0110VBE","VOLKSWAGEN","Golf","VW370-00-0073",0,1.395,3155,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","LVGA10061705","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.015000000000000001,0.02,"0.20",0,"Volkswagen: Jetta"]
[2020,"Volkswagen Group of","LVGAV02.9N7S","LVGAR0150NCS","AUDI","A8L","KN7M-D5",0,2.995,4806,null,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KVGA10055600","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.184,0.20900000000000002,"0.300",0.025,"Audi: S6, S7"]
[2020,"Volkswagen Group of","LVGAV05.2NBE","LVGAR0155NAL","AUDI","R8","LNBE-R8B",2,5.204000000000001,3968,null,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","LVGA10058209","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.005,0.011000000000000001,"0.200",0.006,"Audi: R8, R8 Spyder"]
[2020,"Volvo","LVVXJ02.0P30","LVVXR0142EP2","Volvo","XC90 T8 AWD","201926",0,1.969,5215,6635,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KVVX10053566","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.050",0,"Volvo Cars of North America, LLC: S60 AWD, S90 AWD, V60 AWD, XC60 AWD, XC90 AWD"]
[2020,"Volvo","LVVXJ02.0U70","LVVXR0142E52","Volvo","XC60 T6 AWD","201812",0,1.969,4268,5475,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVVX10047777","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.008,0.008,"0.200",0,"Volvo Cars of North America, LLC: V60 CC AWD, XC60 AWD"]
[2020,"Volvo","LVVXV02.0P3R","LVVXR0142EP2","Volvo","XC90 T8 AWD","201926",0,1.969,5215,6635,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","KVVX10053563","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1752,0.197,"0.300",0.022000000000000002,"Polestar Automotive USA Inc: Polestar 1"]
[2019,"BMW","KBMXJ03.0F16","KBMXR0130N54","BMW","335i xDrive","KS33736",0,3,3825,4883,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000612","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.012,0.01,"0.05",2E-3,"BMW: 640i Gran Coupe, 640i xDrive Gran Coupe"]
[2019,"BMW","KBMXJ04.4N63","KBMXR0180G05","BMW","X5 xDrive50i","LB15156",0,4.4,5170,6460,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KBMX91003985","EPA","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.27240000000000003,0.302,"0.500",0.0297,"BMW: X5 xDrive50i, X7 xDrive50i"]
[2019,"BMW","KBMXV02.0B46","KBMXR0100F5X","Mini","Mini Cooper (5-doors)","T826907",0,1.5,2815,3750,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FBMX10033197","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.04,0.04,"0.05",0,"Mini: COOPER S CONVERTIBLE, COOPER S HARDTOP 2 DOOR, COOPER S HARDTOP 4 DOOR"]
[2019,"BMW","KBMXV02.0M48","KBMXR0100F56","Mini","Mini Cooper (3-doors)","T730204",0,1.5,2675,3520,3000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EBMX10029400","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.058,0.11,"0.20",0.054,"Mini: JOHN COOPER WORKS CONVERTIBLE, JOHN COOPER WORKS HARDTOP"]
[2019,"BMW","KBMXV03.0B2X","KBMXR0130F3X","BMW","330i","5D42601",0,2,3541,4530,3875,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10042334","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.131,0.13,"0.20",2E-3,"BMW: M240i Convertible, M240i Coupe, M240i Coupe M Performance, M240i xDrive Convertible, M240i xDrive Coupe, M240i xDrive Coupe M Performance"]
[2019,"FCA US LLC","KCRXD06.45V2","KCRXR0272TC1","Dodge","RAM 1500 PICKUP 4WD","V3DR10673",0,3.7,4858,6650,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","8CRX01051891","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.4,0.4,"1.4",0,"RAM: 2500 4X2, 2500 4X4"]
[2019,"FCA US LLC","KCRXJ01.45P0","KCRXR0100PK0","Fiat","500","L2FFF2534",0,1.4000000000000001,2421,3300,2750,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N","CCRX10011972","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.045000000000000005,0.04,"0.20",0,"FIAT: 500, 500 Abarth"]
[2019,"FCA US LLC","KCRXT02.05P1","KCRXR0136PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050401","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2922,0.301,"0.375",0.009000000000000001,"Jeep: Wrangler 4X4"]
[2019,"FCA US LLC","KCRXT02.45P1","KCRXR0118PP0","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043879","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"Jeep: Cherokee 4X4, Cherokee FWD"]
[2019,"FCA US LLC","KCRXT02.45P4","KCRXR0110PP0","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043880","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2414,0.25,"0.300",0.009000000000000001,"Jeep: Renegade 4x2, Renegade 4x4"]
[2019,"FCA US LLC","KCRXT03.65P6","KCRXR0125FEH","Chrysler","Pacifica Hybrid","L7RUE4638",0,3.6,5021,6300,5250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HCRX10045055","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chrysler: Pacifica Hybrid"]
[2019,"FCA US LLC","KCRXT03.65P7","KCRXR0172PP0","Jeep","Wrangler Unlimited 4X4","L8JLJ2008",1,3.6,4258,5300,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10050402","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.038,0.04,"0.20",0,"Jeep: Wrangler Unlimited 4X4"]
[2019,"FCA US LLC","KCRXT05.75P1","KCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049386","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2019,"FCA US LLC","KCRXT05.7FP6","KCRXR0183RP0","RAM","1500 4X4","V7DS61975",0,3.6,5292,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX10049483","MFR","24","Federal fuel refueling test (ORVR)","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.03,0.03,"0.20",0,"RAM: 1500 Classic 4X2, 1500 Classic 4X4"]
[2019,"FCA US LLC","KCRXT05.7FP6","KCRXR0225RP0","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4176,0.42300000000000004,"0.500",0.0057,"RAM: 1500 Classic 4X2, 1500 Classic 4X4"]
[2019,"Ferrari","KFEXV03.9TUR","KFEXR0175149","Ferrari","GTC4Lusso T","218129",0,3.9,4178,5313,4750,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","JFEX10045795","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.013000000000000001,0.01,"0.05",0,"Ferrari North America, Inc.: 488 Pista, 488 Pista Spider, 488 Spider, 488 gtb, GTC4Lusso T, Portofino"]
[2019,"FOMOCO","KFMXD03.76BK","KFMXF0190NBS","Ford","T350 FFV Van","ETH1-3.7-J-465",0,3.7,6925,9500,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10028137","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.35000000000000003,0.4,"001.4",0,"Ford: TRANSIT T250 CHASSIS CAB 2WD FFV, TRANSIT T250 CUTAWAY 2WD FFV, TRANSIT T350 CHASSIS CAB 2WD FFV, TRANSIT T350 CUTAWAY 2WD FFV"]
[2019,"FOMOCO","KFMXD03.77BX","KFMXR0190NBS","Ford","T350 FFV Van","ETH1-3.7-J-465",0,3.7,6925,9500,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10028137","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.35400000000000004,0.35000000000000003,"1.00",0,"Ford: TRANSIT T350 VAN, TRANSIT T350 WAGON"]
[2019,"FOMOCO","KFMXJ03.5VEP","KFMXR0145GBC","FORD","FLEX","AP33-3.5-J-566",0,3.5,4964,6250,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","AFMX10002632","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.016,0.02,"0.20",0,"Ford: EXPLORER AWD, Interceptor Utility AWD"]
[2019,"FOMOCO","KFMXT02.01B2","KFMXR0090GDE","Ford","EcoSport","JBW1-2.0-J-073",1,2,3389,4253,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JFMX10049005","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",1E-3,0,"0.05",0,"Ford: ECOSPORT AWD"]
[2019,"FOMOCO","KFMXT02.32ED","KFMXR0125NBB","Ford","Escape AWD","DM21-1.6-F-223",0,1.6,3714,4770,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DFMX10018866","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.008,0.01,"000.20",0,"Lincoln: MKC  AWD"]
[2019,"FOMOCO","KFMXT02.52FB","KFMXR0130NDF","Ford","Transit Connect FWD","GHC1-2.5-C-753",1,2.5,3968,5280,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HFMX10047600","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",8.6E-3,0.009000000000000001,"0.020",0,"Ford: ESCAPE FWD"]
[2019,"FOMOCO","KFMXT03.53E8","KFMXR0145GBC","FORD","FREESTYLE AWD","8P51-3.5-F-509",4,3.5,4431,5460,4750,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","AFMX10001952","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Ford: EXPLORER AWD, EXPLORER FWD"]
[2019,"FOMOCO","KFMXT03.54JK","KFMXR0260NDP","Ford","F-150","JFC1-2.7-J-027",0,2.7,4903,7000,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047784","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2084,0.20800000000000002,"0.500",0,"Ford: F150 2WD BASE PAYLOAD LT TIRE, F150 3.5L 2WD GVWR>7599 LBS, F150 3.5L 4WD GVWR>7599 LBS, F150 4WD BASE PAYLOAD LT TIRE, F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2019,"FOMOCO","KFMXT03.54JM","KFMXR0260NDX","Ford","F-150 4X4 SUPER CREW CAB","JKC00022",0,2.7,4925,6600,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KFMX10057896","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",4.8000000000000004E-3,0.005,"0.020",0,"Ford: F150 PICKUP 2WD LIMITED, F150 PICKUP 4WD LIMITED, F150 RAPTOR 4WD"]
[2019,"FOMOCO","KFMXV02.0VZ7","KFMXR0145HCE","Ford","Fusion (PHEV)","HC71-2.0-J-810",0,2,3972,4910,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HFMX10040110","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.019,0.03,"0.20",0.013000000000000001,"Ford: FUSION POLICE RESPONDER HEV"]
[2019,"FOMOCO","KFMXV02.5VEU","KFMXR0130NDE","Ford","FUSION FWD","HR100020",2,2.5,3475,4430,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","JFMX10045869","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2116,0.21200000000000002,"0.300",0,"Ford: FUSION FWD"]
[2019,"FOMOCO","KFMXV03.5VGT","KFMXR0125NAA","Ford","GT","HS105006",0,3.5,3352,3700,3625,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"Y","N",null,null,"N","HFMX10044599","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",2E-3,"Ford: FORD GT"]
[2019,"GM","KGMXD06.0395","KGMXR021260A","GMC","K35 SIERRA 4WD","60CPHNT892",0,6,7030,11000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10042138","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.014,0.01,"0.20",0,"Chevrolet: C25 SILVERADO 2WD, C35 SILVERADO 2WD, K25 SILVERADO 4WD, K35 SILVERADO 4WD  GMC: C25 SIERRA 2WD, C35 SIERRA 2WD, K25 SIERRA 4WD, K35 SIERRA 4WD"]
[2019,"GM","KGMXD06.0398","KGMXF0223850","CHEVROLET","K35 CHEV CAB CHASSIS 4WD","60XEKCB966",0,6,11300,13200,12000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10037049","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0,0,"0.05",0,"Chevrolet: C35 CHEV CAB CHASSIS 2WD, C35 SILVERADO 2WD, K35 CHEV CAB CHASSIS 4WD, K35 SILVERADO 4WD  GMC: C35 GMC CAB CHASSIS 2WD, C35 SIERRA 2WD, K35 GMC CAB CHASSIS 4WD, K35 SIERRA 4WD"]
[2019,"GM","KGMXT02.0300","KGMXR0146845","CHEVROLET","TRAVERSE","201JNN5404",0,2,4326,6173,4750,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","JGMX10048252","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL-EQUIV",0.049,0.05,"0.20",0,"Chevrolet: TRAVERSE"]
[2019,"GM","KGMXT02.5201","KGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040175","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: BLAZER FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2019,"GM","KGMXT03.6151","KGMXR014640A","GMC","ACADIA AWD","25THNN5072",0,2.5,4213,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040174","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.343,0.343,"0.450",0,"Buick: ENCLAVE, ENCLAVE AWD  Cadillac: XT5, XT5 AWD  Chevrolet: BLAZER AWD, BLAZER FWD, TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2019,"GM","KGMXT05.3385","KGMXR017350D","GMC","C15 SIERRA 2WD","43CPHN1208",0,4.3,4839,6500,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040903","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.011000000000000001,0.01,"0.20",0,"Chevrolet: C10 SILVERADO 2WD, C10 SILVERADO 2WD CAB CHASSIS, K10 SILVERADO 4WD, K10 SILVERADO 4WD CAB CHASSIS  GMC: C10 SIERRA 2WD, C10 SIERRA 2WD CAB CHASSIS, K10 SIERRA 4WD, K10 SIERRA 4WD CAB CHASSIS"]
[2019,"GM","KGMXT05.3386","KGMXR017350D","GMC","C15 SIERRA 2WD","43CPHN1208",0,4.3,4839,6500,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10051772","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.0073,0.007,"0.020",0,"Chevrolet: C10 SILVERADO 2WD, C10 SILVERADO 2WD CAB CHASSIS, K10 SILVERADO 4WD, K10 SILVERADO 4WD CAB CHASSIS, K10 SILVERADO 4WD TRAILBOSS  GMC: C10 SIERRA 2WD, C10 SIERRA 2WD CAB CHASSIS, K10 SIERRA 4WD, K10 SIERRA 4WD AT4, K10 SIERRA 4WD CAB CHASSIS"]
[2019,"GM","KGMXV01.5010","KGMXR011030C","CHEVROLET","MALIBU","151GZN4064",0,1.5,3334,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10038626","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Chevrolet: MALIBU"]
[2019,"GM","KGMXV01.8050","KGMXR0102815","CHEVROLET","MALIBU","181GZN4162",0,1.8,3369,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","GGMX10040165","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.34600000000000003,0.35000000000000003,"0.50",0,"Chevrolet: MALIBU"]
[2019,"GM","KGMXV03.6042","KGMXR0120818","CHEVROLET","MALIBU","181GZN4162",0,1.8,3369,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","GGMX10040163","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.366,0.37,"0.65",0,"Cadillac: ATS-V"]
[2019,"GM","KGMXV03.6165","KGMXR013030B","CADILLAC","CTS AWD","206GAE4665",0,2,3947,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JGMX10051643","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.017,0.017,"0.020",0,"Cadillac: CTS, CTS AWD  Chevrolet: CAMARO"]
[2019,"GM","KGMXV03.6167","KGMXR0133810","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017013","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.20500000000000002,0.2,"0.50",0,"Cadillac: XTS HEARSE, XTS LIMO"]
[2019,"Honda","KHNXT02.0823","KHNXR01491SA","ACURA","RDX AWD A-SPEC","EKYF4A",0,2,4087,5027,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","KHNX10052113","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1784,0.17800000000000002,"0.400",0,"Acura: RDX AWD, RDX FWD"]
[2019,"Honda","KHNXT03.5J53","KHNXR01502SA","HONDA","ODYSSEY FWD","EHMR3A",0,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10046195","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",null,"Honda: ODYSSEY FWD"]
[2019,"Honda","KHNXV01.54K2","KHNXR0127VSB","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044298","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0044,0.004,"0.020",0,"Honda: ACCORD"]
[2019,"Honda","KHNXV01.5SH2","KHNXR0113VSB","HONDA","CIVIC 4DR SEDAN 1.5L","EGAA4C",0,1.5,2908,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10037941","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2179,0.218,"0.300",0,"Honda: CIVIC 5Dr"]
[2019,"Honda","KHNXV02.0BL2","KHNXR0121VSA","HONDA","CR-V 2.4L","EHPH2C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HHNX10044435","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2016,0.202,"0.300",0,"Honda: ACCORD"]
[2019,"Honda","KHNXV03.5MH4","KHNXR0151VFA","ACURA","RLX","EJ9P2A",0,3.5,3977,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JHNX10048468","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.222,0.25,"0.50",0.03,"Acura: RLX"]
[2019,"Hyundai","KHYXV01.4CD6","KHYXR0130CDG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038647","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.0056,0.006,"0.020",0,"HYUNDAI MOTOR COMPANY: Elantra"]
[2019,"Hyundai","KHYXV01.6EC5","KHYXR0143ECG","HYUNDAI","Sonata","LF5F0TU51A1",0,2,3505,4630,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FHYX10040735","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","3Z","California LEV-III Zero Evap (Option 1)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.02,"0.20",0,"HYUNDAI MOTOR COMPANY: Sonata"]
[2019,"Hyundai","KHYXV02.0BG6","KHYXR0110BGE","HYUNDAI","Accent","RB1R6GU05A1",0,1.6,2522,3549,2875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CHYX10012074","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.29400000000000004,0.29,"0.65",0,"HYUNDAI MOTOR COMPANY: Veloster N"]
[2019,"Hyundai","KHYXV02.0CE5","KHYXR0130CEG","Hyundai","Elantra","AD7N0GU03AC",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038455","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.006,0.01,"0.20",2.1000000000000003E-3,"HYUNDAI MOTOR COMPANY: Elantra, Elantra SE"]
[2019,"Hyundai","KHYXV02.0EG5","KHYXR0143EGG","HYUNDAI","Sonata","LF5F0TU51A1",0,2,3505,4630,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FHYX10040737","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","3Z","California LEV-III Zero Evap (Option 1)","150","LEAK-DIA",0,0,"0.02",0,"HYUNDAI MOTOR COMPANY: Sonata"]
[2019,"Hyundai","KHYXV02.4EH3","KHYXR0143EGG","HYUNDAI","Sonata","LF5F0TU51A1",0,2,3505,4630,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FHYX10040735","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","3Z","California LEV-III Zero Evap (Option 1)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.02,"0.20",0,"HYUNDAI MOTOR COMPANY: Sonata, Sonata SE"]
[2019,"Hyundai","KHYXV02.4LH5","KHYXR0133LHG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10038282","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.004,0,"0.20",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2019,"Hyundai","KHYXV03.3NJF","KHYXR0135NJE","Hyundai","Santa Fe","NC3L3AU05A2",0,3.3000000000000003,4184,5622,4500,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","DHYX10022513","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.013000000000000001,0.01,"0.05",0,"HYUNDAI MOTOR COMPANY: Santa Fe XL AWD, Santa Fe XL FWD, Santa Fe XL Ultimate AWD, Santa Fe XL Ultimate FWD"]
[2019,"Jaguar Land Rover L","KJLXJ03.0FSP","KJLXR0160P1Z","Jaguar","XJ","2DFLVP35",0,3,4287,5235,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","FJLX10031802","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL",0.2286,0.23800000000000002,"0.300",0.009000000000000001,"Jaguar: F-TYPE Convertible, F-TYPE Convertible Manual, F-TYPE Coupe, F-TYPE Coupe Manual, F-TYPE S AWD Convertible, F-TYPE S AWD Coupe, F-TYPE S Convertible, F-TYPE S Convertible Manual, F-TYPE S Coupe, F-TYPE S Coupe Manual, XE, XE AWD, XF, XF AWD, XF Sportbrake AWD, XJ, XJ AWD, XJL, XJL AWD"]
[2019,"Kia","KKMXT02.4HH3","KKMXR0133HHG","HYUNDAI","Tucson","TL6N0HU03AC",0,2,3489,4740,3750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GHYX10034920","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.012,0.01,"0.05",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FE AWD, Sportage FE FWD, Sportage FWD"]
[2019,"Kia","KKMXT03.3KJ5","KKMXR0139KJG","KIA","SEDONA","YP9L3AU07AC",0,3.3000000000000003,4740,6085,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KKMX10050566","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.006,0.01,"0.05",0.004,"KIA MOTORS CORPORATION: Sedona"]
[2019,"Kia","KKMXV01.6BA6","KKMXR0110BAG","Kia","Soul","PS7N0AU01AC",0,2,3117,4101,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX91003149","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.18630000000000002,0.186,"0.300",0,"KIA MOTORS CORPORATION: Soul"]
[2019,"Kia","KKMXV02.0CE3","KKMXR0130CEG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038653","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",0,0,"0.020",0,"KIA MOTORS CORPORATION: Forte, Forte FE"]
[2019,"Kia","KKMXV02.0D2T","KKMXR0125D2E","HYUNDAI","SONATA PLUG-IN HYBRID","PLF5NAUP12A",0,2,3810,4784,4000,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"Y","GHYX10036575","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.018000000000000002,0.02,"0.20",0.005,"KIA MOTORS CORPORATION: Optima plug-in hybrid"]
[2019,"Kia","KKMXV02.4JH5","KKMXR0132JHG","Kia","Sorento","UM9L3AU01AC",0,3.3000000000000003,4303,5622,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KKMX10050506","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2127,0.215,"0.300",2.1000000000000003E-3,"KIA MOTORS CORPORATION: Sorento AWD, Sorento FWD"]
[2019,"Maserati","KMAXT03.0AWD","KMAXR0110161","MASERATI","QUATTROPORTE GTS","070989",1,3.8000000000000003,4495,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","HMAX10042289","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.2",0.01,"MASERATI: LEVANTE, LEVANTE S"]
[2019,"Maserati","KMAXV04.7LEV","KMAXR0198138","MASERATI","QUATTROPORTE","ZAMCD39B000010379",0,4.2,4376,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"N","N","SF","Single Fuel","N","AMAX10005370","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.015000000000000001,0.02,"0.05",1E-3,"MASERATI: GRANTURISMO CONVERTIBLE"]
[2019,"McLaren Automotive ","KMLNV03.8M13","KMLNR0164M13","McLaren","MP4-12C Coupe","SBM11BAA0AW99PP06",0,3.798,3181,3688,3500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"N","N",null,null,"N","CMLN10017329","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","150","HC",0.026000000000000002,0.03,"0.05",0,"McLaren: 540C Coupe, 570GT, 570S Coupe, 570S Spider, 600LT Coupe, 600LT Spider"]
[2019,"Mercedes-Benz","KMBXJ02.0U2C","KMBXR0155LNC","Mercedes-Benz","C 300 4MATIC","Z5023",0,1.991,3715,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10048286","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","4","HC-TOTAL",0.014,0.014,"0.020",0,"Mercedes-Benz: E 300, E 300 4MATIC, GLC 300, GLC 300 4MATIC, GLC 300 4MATIC (Coupe)"]
[2019,"Mercedes-Benz","KMBXT02.0HY1","KMBXR0155LNP","Mercedes-Benz","C350e","W205-P2-60-Z6004",0,1.991,4175,5082,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"Y","GMBX10044535","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","B","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1512,0.151,"0.275",0,"Mercedes-Benz: GLC 350e 4MATIC"]
[2019,"Mercedes-Benz","KMBXV02.0U2C","KMBXR0110LNF","Mercedes-Benz","B 250","W246E20DETC-Z3021",0,1.991,3293,4409,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,7,"Y","N",null,null,"N","DMBX10023101","MFR","24","Federal fuel refueling test (ORVR)","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.024,0.05,"0.20",0.022000000000000002,"Mercedes-Benz: AMG CLA 45 4MATIC, AMG GLA 45 4MATIC"]
[2019,"Mercedes-Benz","KMBXV03.0U2A","KMBXR0170LNS","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10048076","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","4","HC-TOTAL",0.017400000000000002,0.017,"0.020",0,"Mercedes-Benz: S 450, S 450 4MATIC, S 450 4MATIC (W)"]
[2019,"Mitsubishi Motors Co","KMTXT02.0G5P","KMTXR0135A1D","MITSUBISHI","LANCER","EB08-CA32",0,1.998,2922,4079,3250,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N","AMTX10003926","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.12100000000000001,0.12100000000000001,"0.650",0,"Mitsubishi Motors Corporation: OUTLANDER SPORT 2WD, RVR 2WD"]
[2019,"Mitsubishi Motors Co","KMTXT02.4G5Y","KMTXR0135A2E","MITSUBISHI","OUTLANDER 2WD","EB18-RB5A",5,2.36,3345,4795,3625,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,6,"Y","N",null,null,"N","JMTX10046917","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.229,0.24300000000000002,"0.3000",0.014,"Mitsubishi Motors Corporation: OUTLANDER 2WD"]
[2019,"Nissan","KNSXT02.0N2A","KNSXR0114PDA","NISSAN","NV200 Cargo Van","KEEJ07",1,2,3301,4773,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","JNSX10048749","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.24500000000000002,0.24500000000000002,"0.300",0,"NISSAN: NV200 Cargo Van"]
[2019,"Nissan","KNSXT02.5R5A","KNSXR0114PEA","NISSAN","ROGUE AWD","BTEL15",0,2.5,3653,4720,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","JNSX10048363","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2666,0.267,"0.400",0,"NISSAN: ROGUE AWD, ROGUE FWD"]
[2019,"Nissan","KNSXT04.0N6A","KNSXR0132PBA","NISSAN","NISSAN FRONTIER 4WD C/C PRO-4X","SRE410",0,4,4567,5599,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N",null,null,"N","DNSX91001595","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.559,0.56,"0.85",0,"NISSAN: FRONTIER 2WD, FRONTIER 4WD"]
[2019,"Nissan","KNSXV01.6NDA","KNSXR0090PBB","NISSAN","NISSAN JUKE AWD SL","KHEH11",0,1.6,3234,null,3500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","FNSX10032170","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"NISSAN: SENTRA, SENTRA NISMO"]
[2019,"Nissan","KNSXV02.0PMA","KNSXR0114PCB","NISSAN","Rogue Sport AWD","BSEH58",0,2,3455,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","KNSX10054154","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"NISSAN: Qashqai, Qashqai AWD, Rogue Sport, Rogue Sport AWD"]
[2019,"Nissan","KNSXV03.0NHA","KNSXR0159MCB","INFINITI","Q50 AWD RED SPORT","HREH71",1,3,4025,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","JNSX10046132","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.21100000000000002,0.21100000000000002,"0.300",0,"INFINITI: Q50, Q50 AWD, Q50 AWD RED SPORT, Q50 RED SPORT, Q60, Q60 AWD, Q60 AWD RED SPORT, Q60 RED SPORT"]
[2019,"Porsche","KPRXT03.0CV6","KPRXR0150RED","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","KPRX10054425","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.009000000000000001,0.009000000000000001,"0.020",0,"Porsche: Cayenne, Cayenne S"]
[2019,"Porsche","KPRXV04.0PH8","KPRXR0170RPH","Porsche","Panamera 4 e-Hybrid Executive","ECFE-971H-18",0,2.9,4960,6117,5500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"Y","JPRX10048012","MFR","23","2-day evap","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","EPAA","EPA Assigned","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1208,0.133,".300",0.0126,"Porsche: Panamera Turbo S e-Hybrid, Panamera Turbo S e-Hybrid Exec, Panamera Turbo S e-Hybrid ST"]
[2019,"Roush","KRIID06.87CV","KRIIF0265LP2","Roush","E350 Cutaway","PE351",0,5.4,6000,9600,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","BRII10007975","MFR","34","Federal fuel 3-day evap","42","LPG","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.33,0.3,"1.4",0,"Roush Industries, Inc.: E350 Cutaway Propane, E350 Strip Chassis Propane"]
[2019,"Subaru","KFJXJ02.5BUY","KFJXR01155AD","SUBARU","IMPREZA 5-Door","HBV-YU15",0,2,3195,4299,3500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N","HFJX10042771","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.24880000000000002,0.253,"0.300",0.0044,"Subaru: IMPREZA 4-Door, IMPREZA 4-Door SPORT, IMPREZA 5-Door, IMPREZA 5-Door SPORT"]
[2019,"Subaru","KFJXJ03.6KTX","KFJXR01473DB","SUBARU","OUTBACK","FBV-XD16",1,3.6,3845,null,4250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","FFJX10029266","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.011000000000000001,0.01,"0.20",0,"Subaru: LEGACY, OUTBACK AWD"]
[2019,"Toyota","KTYXT02.5P3N","KTYXR0165J82","TOYOTA","RAV4 HYBRID AWD","19-AA1H",0,2.487,3800,4920,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"N","N",null,null,"Y","KTYX10056194","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1589,0.159,"0.400",0,"TOYOTA: RAV4 HYBRID AWD"]
[2019,"Toyota","KTYXT03.5M5N","KTYXR0165P82","TOYOTA","SIENNA AWD","17-GL4A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","HTYX10041743","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.23040000000000002,0.23,"0.400",0,"TOYOTA: TACOMA 2WD, TACOMA 4WD, TACOMA 4WD D-CAB V6 MT OFF-ROAD, TACOMA 4WD TRD PRO"]
[2019,"Toyota","KTYXT04.6B6X","KTYXR0190P32","TOYOTA","TOYOTA TUNDRA 4WD","09-SK3A",0,5.663,5760,7200,6000,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9TYX01085296","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.558,0.59,"1.15",0.035,"LEXUS: GX 460"]
[2019,"Toyota","KTYXV01.5B6B","KTYXR0085P12","SCION","iQ","11-NJ2C",0,1.329,2135,null,2375,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N","SF","Single Fuel","N","BTYX10009641","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",1E-3,0,"0.05",0,"TOYOTA: YARIS"]
[2019,"Toyota","KTYXV01.8M5B","KTYXR0115P12","TOYOTA","COROLLA MATRIX","05-ZE4",0,1.796,2865,null,3125,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N","SF","Single Fuel","N","5TYX01055681","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","150","HC-TOTAL",0.228,0.26,"0.50",0.035,"TOYOTA: COROLLA LE ECO"]
[2019,"Toyota","KTYXV02.5P35","KTYXR0165J72","TOYOTA","CAMRY HYBRID XLE/SE","18-AV3H",0,2.487,3565,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","JTYX10047603","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1658,0.166,"0.300",0,"TOYOTA: CAMRY HYBRID LE"]
[2019,"Toyota","KTYXV03.5M5B","KTYXR0130P72","TOYOTA","CAMRY XLE/XSE","18-AV1A",1,2.487,3415,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","JTYX10046252","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.005,0,"0.05",0,"LEXUS: ES 350, ES 350 F SPORT  TOYOTA: AVALON, AVALON XLE, CAMRY, CAMRY XSE"]
[2019,"Volkswagen Group of","KVGAJ03.0N7F","KVGAR0140NCP","AUDI","A4","HAAC-BAQ",4,1.984,4035,null,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","HVGA10045302","MFR","32","Federal Fuel Running Loss","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,1E-3,"0.050",1E-3,"Audi: RS 5, RS 5 Sportback, S4, S5, S5 Cabriolet, S5 Sportback"]
[2019,"Volkswagen Group of","KVGAT02.0AAA","KVGAR0135VCS","VOLKSWAGEN","Atlas","VW416070129",0,3.6,4713,5732,5000,"A","All Wheel Drive","A","Automatic",null,8,"Y","N",null,null,"N","JVGA10046317","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.015700000000000002,0.016,"0.020",0,"Volkswagen: Atlas"]
[2019,"Volkswagen Group of","KVGAV01.8APA","KVGAR0110ABB","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3-3Z","Federal Tier 3 LEV-III Zero Evap (Option 1) Carryover","150","HC-TOTAL",0.26,0.274,"0.350",0.014,"Audi: A3 Cabriolet quattro  Volkswagen: Golf Alltrack, Golf SportWagen 4Motion"]
[2019,"Volkswagen Group of","KVGAV02.5NAG","KVGAR0110AAA","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX10001963","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Audi: RS 3, TT RS"]
[2019,"Volkswagen Group of","KVGAV05.2NDE","KVGAR0155NAL","AUDI","R8","8375-RAQ",1,4.163,3671,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01076742","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.273,0.29,"0.650",0.017,"Lamborghini: Huracan, Huracan Spyder"]
[2019,"Volvo","KVVXJ02.0U7A","KVVXR0142EV5","Volvo","XC60 T6 AWD","201812",0,1.969,4268,5475,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVVX10047697","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2005,0.21100000000000002,"0.300",0.0106,"Volvo Cars of North America, LLC: S60 FWD, S90 AWD, S90 FWD, V60 CC AWD, V60 FWD, V90 CC AWD, V90 FWD, XC60 AWD, XC60 FWD"]
[2018,"aston martin","JASXV06.0VHB","JASXR0160P1Y","Aston Martin","DB9","VIN132",0,5.9,4090,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","5ASX01059906","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.01,0,"0.2",0,"Aston Martin Lagonda Ltd: Rapide S, Vanquish, S and Zagato"]
[2018,"BMW","JBMXJ02.0N20","JBMXR0130N54","BMW","335i xDrive","KS33736",0,3,3825,4883,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX01071568","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.308,0.31,"0.50",0.006,"BMW: 320i, 320i xDrive, X4 xDrive28i"]
[2018,"BMW","JBMXV01.5H60","JBMXR0140G3H","BMW","530e xDrive","G623301",0,2,4385,5470,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y","JBMX10045981","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2315,0.264,"0.300",0.032100000000000004,"Mini: MINI COOPER SE COUNTRYMAN ALL4"]
[2018,"BMW","JBMXV01.5M3X","JBMXR0130F45","Mini","Mini Cooper Countryman","3B62508",0,1.5,3360,4376,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HBMX10043378","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.006,0.01,"0.05",0,"Mini: COOPER CLUBMAN ALL4, COOPER COUNTRYMAN, COOPER COUNTRYMAN ALL4"]
[2018,"BMW","JBMXV03.0B2X","JBMXR0130F3X","BMW","330i","5D42601",0,2,3541,4530,3875,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10042276","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","4","HC-TOTAL-EQUIV",0.0032,0.003,"0.020",null,"BMW: M240i Coupe, M240i xDrive Coupe"]
[2018,"BMW","JBMXV03.0B58","JBMXR0170N63","BMW","750i","CY33005",0,4.4,4641,5788,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000808","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.028,0.03,"0.05",0,"BMW: 740i, 740i xDrive"]
[2018,"FCA US LLC","JCRXD06.45V2","JCRXF0272TC0","Dodge","RAM 1500 PICKUP 4WD","V3DR10673",0,3.7,4858,6650,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","8CRX01051890","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.33,0.33,"1.25",0,"RAM: 2500 Cab Chassis 4X2, 2500 Cab Chassis 4X4"]
[2018,"FCA US LLC","JCRXJ01.45P0","JCRXR0107PK1","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017734","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"FIAT: 124 Spider"]
[2018,"FCA US LLC","JCRXJ02.05P0","JCRXR0107PK0","Alfa Romeo","Stelvio AWD","L7GUF8294",0,2,4030,5247,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003488","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","F2","Federal LEV-II Evap","150","HC-TOTAL",0.278,0.29,"0.65",0.01,"ALFA ROMEO: Stelvio AWD"]
[2018,"FCA US LLC","JCRXT02.45P1","JCRXR0118FE2","Dart","Dodge","L4PFD6873",1,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10029389","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T3-3Z","Federal Tier 3 LEV-III Zero Evap (Option 1) Carryover","150","HC-TOTAL",0.2326,0.273,"0.500",0.04,"Jeep: Cherokee 4X4, Cherokee 4x4 Active Drive II, Cherokee FWD, Cherokee Trailhawk 4X4"]
[2018,"FCA US LLC","JCRXT02.45PA","JCRXR0118PPB","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043880","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2414,0.25,"0.400",0.009000000000000001,"Jeep: Cherokee 4X4, Cherokee FWD"]
[2018,"FCA US LLC","JCRXT03.65P4","JCRXR0140RP0","Chrysler","Pacifica","L7RUC8881",0,3.6,5189,6005,5250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N","HCRX10044760","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.34700000000000003,0.35300000000000004,"0.500",0.006,"Chrysler: Pacifica"]
[2018,"FCA US LLC","JCRXT03.65PB","JCRXR0225RPA","RAM","1500 4X4","V7DS61972",0,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","JCRX91003631","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4176,0.42400000000000004,"0.500",0.006,"RAM: 1500 4X2, 1500 4X4"]
[2018,"FCA US LLC","JCRXT06.25P1","JCRXR0180RK0","Jeep","Grand Cherokee 4wd","K1WKJ8647",0,3.6,4716,6500,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BCRX10008678","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.115,0.14,"0.20",0.02,"Jeep: Grand Cherokee TrackHawk 4x4"]
[2018,"FCA US LLC","JCRXT06.25P1","JCRXR0180RK0","Jeep","Grand Cherokee 4wd","K1WKJ8647",0,3.6,4716,6500,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BCRX10008679","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Jeep: Grand Cherokee TrackHawk 4x4"]
[2018,"Ferrari","JFEXV06.5GDI","JFEXR017512C","Ferrari","812 Superfast","021680",0,6.5,3858,4475,4250,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","JFEX10047180","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.34900000000000003,0.35000000000000003,"0.50",0,"Ferrari North America, Inc.: 812 Superfast, GTC4Lusso"]
[2018,"FOMOCO","JFMXD03.76BK","JFMXF0190NBS","Ford","T350 FFV Van","ETH1-3.7-J-465",0,3.7,6925,9500,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10028135","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.329,0.33,"001.75",0,"Ford: TRANSIT T250 CHASSIS CAB 2WD FFV, TRANSIT T250 CUTAWAY 2WD FFV, TRANSIT T350 CHASSIS CAB 2WD FFV, TRANSIT T350 CUTAWAY 2WD FFV"]
[2018,"FOMOCO","JFMXD06.27CH","JFMXF0265NAS","Ford","F350 Incomplete 4x4","BFA1-6.2-J-006",0,6.2,10603,12600,11000,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","BFMX10006406","MFR","15","Spitback","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","SPITBACK",0.46,0.5,"001.0",0,"Ford: F350 INCOMPLETE 2WD FFV, F350 INCOMPLETE 4WD FFV"]
[2018,"FOMOCO","JFMXT01.01B1","JFMXR0090GDE","Ford","EcoSport","JBW1-2.0-J-073",1,2,3389,4253,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JFMX10049001","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.044000000000000004,0.08,"0.20",0.039,"Ford: ECOSPORT FWD"]
[2018,"FOMOCO","JFMXT02.01B2","JFMXR0090GDE","Ford","EcoSport","JBW1-2.0-J-073",1,2,3389,4253,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JFMX10049005","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.05",0,"Ford: ECOSPORT AWD"]
[2018,"FOMOCO","JFMXT02.52K9","JFMXR0130NDF","Ford","Transit Connect FWD","GHC1-2.5-C-753",0,2.5,3968,5280,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GFMX10040107","MFR","24","Federal fuel refueling test (ORVR)","59","Tier 3 E10 Premium Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.027,0.03,"000.20",0.005,"Ford: TRANSIT CONNECT WAGON FWD, Transit Connect Van 2WD, Transit Connect Wagon LWB FWD"]
[2018,"FOMOCO","JFMXT02.73JK","JFMXR0260NDG","Ford","F-150","JFC1-2.7-J-027",0,2.7,4903,7000,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10048126","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.008,0.008,"0.020",0,"Ford: F150 2.7L 2WD GVWR>6649 LBS, F150 2.7L 4WD GVWR>6799 LBS, F150 2WD BASE PAYLOAD LT TIRE, F150 4WD BASE PAYLOAD LT TIRE, F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2018,"FOMOCO","JFMXT03.54JK","JFMXR0260NDG","Ford","F-150","JFC1-2.7-J-027",0,2.7,4903,7000,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047783","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.25370000000000004,0.254,"0.500",0,"Ford: F150 2WD BASE PAYLOAD LT TIRE, F150 3.5L 2WD GVWR>7599 LBS, F150 3.5L 4WD GVWR>7599 LBS, F150 4WD BASE PAYLOAD LT TIRE, F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2018,"FOMOCO","JFMXT03.54JM","JFMXR0200GDG","Ford","F-150","JFC1-2.7-032",0,2.7,4903,7000,5250,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N","JFMX10047782","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"0.05",0,"Ford: F150 RAPTOR 4WD"]
[2018,"FOMOCO","JFMXT03.73E8","JFMXR0145GBC","FORD","FREESTYLE AWD","8P51-3.5-F-509",4,3.5,4431,5460,4750,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","AFMX01073444","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.34900000000000003,0.35000000000000003,"1.15",0,"Ford: EXPLORER AWD, EXPLORER FWD, Interceptor Utility AWD"]
[2018,"FOMOCO","JFMXV01.6VDD","JFMXR0105GBA","Ford","FIESTA","ECT3-1.6-J-404",0,1.6,2631,3620,3000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EFMX10023106","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.005,0,"0.20",0,"Ford: Fiesta ST FWD"]
[2018,"FOMOCO","JFMXV02.0VZT","JFMXR0145HCE","Lincoln","MKZ (HEV)","HC91-2.0-J-815",0,2,3919,4910,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HFMX10040105","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1751,0.17500000000000002,"0.300",0,"Ford: C-MAX Hybrid FWD, FUSION HYBRID FWD  Lincoln: MKZ HYBRID FWD"]
[2018,"FOMOCO","JFMXV03.7VE8","JFMXR0145GBA","FORD","FREESTYLE AWD","8P51-3.5-F-509",4,3.5,4431,5460,4750,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","AFMX01073447","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.34890000000000004,0.34900000000000003,"0.500",0,"Ford: FLEX AWD, Flex FWD, Police Interceptor Sedan AWD, Police Interceptor Sedan FWD, TAURUS AWD, TAURUS FWD  Lincoln: MKT FWD, MKT LIVERY AWD"]
[2018,"GM","JGMXD04.3392","JGMXF0176860","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60XEPGB823",0,6,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10037052","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL-EQUIV",0.29600000000000004,0.3,"1.25",0,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH"]
[2018,"GM","JGMXD06.0395","JGMXR0223841","CHEVROLET","K35 SILVERADO 4WD LONG BOX","60XEKPB999",1,6,7324,13000,7500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","CGMX10012746","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.447,0.45,"1.25",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD PASS  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD PASS"]
[2018,"GM","JGMXT01.5090","JGMXR009537C","CHEVROLET","EQUINOX","151JXV5723",0,1.5,3543,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","JGMX10045841","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN"]
[2018,"GM","JGMXT02.0100","JGMXR009537C","CHEVROLET","EQUINOX","151JXV5723",0,1.5,3543,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","JGMX10045842","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2011,0.201,"0.400",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN, TERRAIN AWD"]
[2018,"GM","JGMXT03.6162","JGMXR013835A","GMC","CANYON 4WD","25SPHN1023",0,2.5,4194,5600,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040907","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.25670000000000004,0.257,"0.400",0,"Chevrolet: COLORADO CAB CHASSIS 2WD, COLORADO ZR2 4WD  GMC: CANYON CAB CHASSIS 2WD"]
[2018,"GM","JGMXT05.3382","JGMXR021250B","CHEVROLET","K15 SILVERADO 4WD","43CPHN1214",0,4.3,4990,6900,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10041700","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.027,0.03,"0.20",0,"Chevrolet: C15 SILVERADO 2WD, C1500 SUBURBAN 2WD, K15 SILVERADO 4WD, K1500 SUBURBAN 4WD  GMC: C15 SIERRA 2WD, C1500 YUKON XL 2WD, K15 SIERRA 4WD, K1500 YUKON XL 4WD"]
[2018,"GM","JGMXT05.3384","JGMXR0223840","GMC","CC15903","43XECP6053",6,4.8,5727,9600,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX10001567","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Chevrolet: C15 SILVERADO 2WD CAB CHASSIS, K15 SILVERADO 4WD CAB CHASSIS  GMC: C15 SIERRA 2WD CAB CHASSIS, K15 SIERRA 4WD CAB CHASSIS"]
[2018,"GM","JGMXV01.6001","JGMXR0120818","CHEVROLET","1ND69","2215NP4000",1,2,3339,4240,3625,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061625","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.58,0.58,"0.65",0,"Buick: CASCADA"]
[2018,"GM","JGMXV02.0031","JGMXR0112830","CHEVROLET","1ND69","2215NP4000",1,2,3339,4240,3625,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX10001983","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Cadillac: CT6"]
[2018,"GM","JGMXV03.6042","JGMXR0112835","CHEVROLET","1ND69","2215NP4000",1,2,3339,4240,3625,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061627","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.025,0.02,"0.20",0,"Cadillac: CT6 AWD"]
[2018,"GM","JGMXV03.6165","JGMXR011030C","CHEVROLET","MALIBU","151GZN4064",0,1.5,3334,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GGMX91002921","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.189,0.19,"0.65",0,"Buick: LACROSSE, LACROSSE AWD, REGAL AWD  Cadillac: ATS, ATS AWD"]
[2018,"GM","JGMXV03.6165","JGMXR0133810","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017014","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Cadillac: XTS, XTS AWD"]
[2018,"Honda","JHNXT03.5GV3","JHNXR01351FA","ACURA","RDX 4WD","ED8A3A",0,3.5,3901,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DHNX10018365","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.42800000000000005,0.44,"0.65",0.01,"Acura: RDX AWD, RDX FWD"]
[2018,"Honda","JHNXV01.5362","JHNXR0113VSB","HONDA","CIVIC 4DR SEDAN 1.5L","EGAA4C",0,1.5,2908,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10037943","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Honda: CIVIC 2Dr, CIVIC 4Dr, CIVIC 5Dr"]
[2018,"Honda","JHNXV02.02H3","JHNXR0113VSB","HONDA","CIVIC 4DR SEDAN 1.5L","EGAA4C",0,1.5,2908,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10037943","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Honda: CIVIC 5Dr"]
[2018,"Honda","JHNXV02.0DH3","JHNXR0113VSA","HONDA","CIVIC 4DR SEDAN 2.0L","EGBB4C",0,2,2808,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10038051","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","120","HC-TOTAL-EQUIV",0.20170000000000002,0.202,"0.300",0,"Honda: CIVIC 2Dr, CIVIC 4Dr"]
[2018,"Honda","JHNXV02.4WH3","JHNXR0121VFA","ACURA","TLX","EFJ24A",0,3.5,3789,null,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","FHNX10031142","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.023,0.03,"0.20",0.01,"Acura: TLX FWD, TLX FWD A-SPEC"]
[2018,"Hyundai","JHYXV01.61F5","JHYXR0140AFG","HYUNDAI","Sonata","LF5F0TU51A1",0,2,3505,4630,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FHYX10040735","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","3Z","California LEV-III Zero Evap (Option 1)","150","HC-TOTAL-EQUIV",0.015000000000000001,0.02,"0.20",0,"HYUNDAI MOTOR COMPANY: Sonata"]
[2018,"Hyundai","JHYXV01.61NF","JHYXR01201NE","Hyundai","Elantra GT","PD8N0AU01AC",0,2,2943,3968,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","JHYX10045179","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.14,0.14,"0.50",0,"HYUNDAI MOTOR COMPANY: Elantra GT"]
[2018,"Hyundai","JHYXV02.01E3","JHYXR01301EG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX91002944","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.19360000000000002,0.194,"0.300",0,"HYUNDAI MOTOR COMPANY: Elantra, Elantra SE"]
[2018,"Hyundai","JHYXV02.41L5","JHYXR01301LE","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10047289","MFR","67","Leak Test - Port Near Canister","58","Tier 3 E10 Regular Gasoline (10 RVP-FFV ORVR Only)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.020",0,"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2018,"Hyundai","JHYXV03.31MF","JHYXR0140ASE","Hyundai","G90","HI7T0AU13AC",0,5,4905,5864,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HHYX10039640","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.024,0.02,"0.05",0,"GENESIS: G90 AWD, G90 RWD"]
[2018,"Jaguar Land Rover L","JJLXT02.0RTV","JJLXR0140P1Z","Land Rover","Range Rover Evoque","3EVPP037",0,2,3995,5181,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","EJLX10028183","MFR","24","Federal fuel refueling test (ORVR)","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.009000000000000001,0.01,"0.20",0,"Jaguar: Jaguar E-Pace  Land Rover: Discovery Sport, Range Rover Evoque, Range Rover Evoque Cabriolet"]
[2018,"Kia","JKMXT02.04MF","JKMXR01304ME","KIA","Sportage","SL1F0HU15A1",0,2,3605,4696,3875,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","BKMX10011579","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.02,0.02,"0.05",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FWD"]
[2018,"Kia","JKMXT03.34SF","JKMXR01354SE","Kia","Sedona SXL","YP5L3U03AC",0,3.3000000000000003,4696,6085,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FKMX10031387","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.02,0.02,"0.20",0,"KIA MOTORS CORPORATION: Sedona, Sedona SX, Sedona SXL"]
[2018,"Kia","JKMXV01.6DA6","JKMXR01104AG","Kia","Soul","PS7N0AU01AC",0,2,3117,4101,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10041747","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2503,0.25,"0.300",0,"KIA MOTORS CORPORATION: Soul"]
[2018,"Kia","JKMXV01.6DDF","JKMXR01284DE","KIA","Forte5","YD3R6AU09A1",0,1.6,3025,4056,3375,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10025129","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.021,0.02,"0.05",0,"KIA MOTORS CORPORATION: Forte Koup, Forte5"]
[2018,"Kia","JKMXV02.04GF","JKMXR01404GG","HYUNDAI","Sonata","LF5F0TU51A1",0,2,3505,4630,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FHYX10029482","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","3Z","California LEV-III Zero Evap (Option 1)","150","HC-TOTAL-EQUIV",0.28700000000000003,0.28700000000000003,"0.350",0,"KIA MOTORS CORPORATION: Optima"]
[2018,"Kia","JKMXV02.44P5","JKMXR0135DWE","Kia","Sorento","UM5F0U09AC",0,2,4169,5247,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GKMX10032901","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.36100000000000004,0.36,"0.50",0,"KIA MOTORS CORPORATION: Sorento AWD, Sorento FWD"]
[2018,"Kia","JKMXV03.84LF","JKMXR0140DLE","KIA","Quoris","KH4L8GU17B2",0,3.8000000000000003,4288,5357,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","FKMX91002024","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.337,0.34,"0.65",0,"KIA MOTORS CORPORATION: K900"]
[2018,"MAZDA","JTKXV02.0CDA","JTKXR0115GCP","MAZDA","MAZDA3","5ECPES1-004",0,2,2919,4001,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FTKX10030648","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"MAZDA: MAZDA3 4-Door, MAZDA3 5-Door"]
[2018,"MAZDA","JTKXV02.5FBA","JTKXR0111GAK","MAZDA","MAZDA6","4EFPY31-004",2,2.5,3183,4226,3500,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N","ETKX10022979","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.155,0.16,"0.50",0.003,"MAZDA: MAZDA3 4-Door, MAZDA3 5-Door"]
[2018,"Mercedes-Benz","JMBXJ03.0U2A","JMBXR0155LNC","Mercedes-Benz","C 300 4MATIC","Z5023",0,1.991,3715,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10037448","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Mercedes-Benz: AMG C 43 4MATIC, AMG C 43 4MATIC (convertible), AMG C 43 4MATIC (coupe), AMG E 43 4MATIC, AMG GLC 43 4MATIC, AMG GLC 43 4MATIC (coupe), E 400 (convertible), E 400 (coupe), E 400 4MATIC, E 400 4MATIC (convertible), E 400 4MATIC (coupe), E 400 4MATIC (station wagon)"]
[2018,"Mercedes-Benz","JMBXJ06.0U2A","JMBXR0155LNS","Mercedes-Benz","SL 600","R230E55TC-Z7019",0,5.513,4519,5095,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","AMBX10002172","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Mercedes-Benz: AMG SL 65"]
[2018,"Mercedes-Benz","JMBXT03.0U2B","JMBXR0170LNF","Mercedes-Benz","GLE 550 4MATIC","W166E46DETC-Z6018",0,4.664000000000001,5200,6500,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","HMBX10039926","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.4544,0.454,"0.475",0,"Mercedes-Benz: AMG GLE 43 4MATIC, AMG GLE 43 4MATIC (coupe), GLE 400 4MATIC, GLS 450 4MATIC"]
[2018,"Mercedes-Benz","JMBXV04.0U2A","JMBXR0155LNA","Mercedes-Benz","AMG C 63 4MATIC","W205E40DETC-Z5020",0,3.982,3928,4883,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10045498","MFR","24","Federal fuel refueling test (ORVR)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.005,0.02,"0.20",0.016,"Mercedes-Benz: AMG C 63, AMG C 63 (convertible), AMG C 63 (coupe), AMG C 63 S, AMG C 63 S (convertible), AMG C 63 S (coupe), AMG E 63 S 4MATIC, AMG E 63 S 4MATIC (Station Wagon"]
[2018,"Mitsubishi Motors Co","JMTXT02.0H3M","JMTXR0148A2L","MITSUBISHI","OUTLANDER PHEV","EB18-RH43",0,1.998,4292,5225,4750,"F","2-Wheel Drive, Front","A","Automatic",null,1,"Y","N",null,null,"Y","JMTX10047881","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0177,0.018000000000000002,"0.200",0,"Mitsubishi Motors Corporation: OUTLANDER PHEV"]
[2018,"Nissan","JNSXT02.0NGA","JNSXR0108PBA","NISSAN","ROGUE AWD Hybrid","BWC280",0,2,3792,4806,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y","HNSX10042924","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.465,0.46,"0.85",0,"NISSAN: ROGUE AWD Hybrid, ROGUE FWD Hybrid"]
[2018,"Nissan","JNSXT02.5R5A","JNSXR0114PCB","NISSAN","ROGUE AWD","BTEL15",0,2.5,3653,4720,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","JNSX10048366","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2748,0.275,"0.400",0,"NISSAN: ROGUE AWD, ROGUE FWD"]
[2018,"Nissan","JNSXT03.5P7A","JNSXR0120PBC","NISSAN","PATHFINDER 4WD PLATINUM","GKB390",1,3.5,4672,5986,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HNSX10041567","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.465,0.46,"0.65",0,"INFINITI: QX60 AWD, QX60 FWD  NISSAN: PATHFINDER 2WD, PATHFINDER 4WD"]
[2018,"Nissan","JNSXV01.6RNA","JNSXR0087PCA","NISSAN","Kicks","HLE425",0,1.6,2634,null,3000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","JNSX10051332","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2419,0.264,"0.300",0.022000000000000002,"NISSAN: Kicks"]
[2018,"Nissan","JNSXV02.5R5A","JNSXR0126PCA","NISSAN","MAXIMA","CNE233",0,3.5,3563,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","JNSX10049124","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.26830000000000004,0.268,"0.300",0,"NISSAN: ALTIMA, ALTIMA SR"]
[2018,"Nissan","JNSXV03.5P7C","JNSXR0120PBA","NISSAN","NISSAN MURANO AWD  SL","JJB066",1,3.5,4041,null,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","FNSX10032246","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"NISSAN: MURANO AWD, MURANO FWD"]
[2018,"Nissan","JNSXV03.8NBA","JNSXR0132MBB","NISSAN","GT-R","MNB211",1,3.8000000000000003,3887,null,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9NSX01081503","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.011000000000000001,0.01,"0.20",0,"NISSAN: GT-R"]
[2018,"Porsche","JPRXT03.6MCS","JPRXR0140RMA","Porsche","Macan S","EC-95BS-15",0,3,4352,5622,4750,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","FPRX10029840","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.023,0.02,"0.20",1E-3,"Porsche: Macan GTS, Macan S"]
[2018,"Porsche","JPRXV04.0T91","JPRXR0150R92","Porsche","911 GT3","FE-991IIGT3-MT-18",0,4,3315,3880,3625,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N","JPRX10049106","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24500000000000002,0.24,"0.65",0,"Porsche: 911 GT2 RS, 911 GT3, 911 GT3 Touring, 911 Turbo, 911 Turbo Cabriolet, 911 Turbo S, 911 Turbo S Cabriolet, 911 Turbo S Exclusive"]
[2018,"Rolls-Royce","JRRGV06.8N74","JRRGR0170RR1","Rolls Royce","Phantom","U105509",0,6.7,5948,7088,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JRRG10048831","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0119,0.012,"0.020",0,"Rolls-Royce Motor Cars Limited: Phantom, Phantom EWB"]
[2018,"Subaru","JFJXJ03.6KTX","JFJXR01473DB","SUBARU","OUTBACK","FBV-XD16",0,3.6,3845,null,4250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","FFJX10029264","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Subaru: LEGACY, OUTBACK"]
[2018,"Toyota","JTYXT02.7B6N","JTYXR0165P82","TOYOTA","SIENNA AWD","17-GL4A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","HTYX10041721","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"TOYOTA: HIGHLANDER"]
[2018,"Toyota","JTYXT02.7M5P","JTYXR0165P82","TOYOTA","SIENNA AWD","17-GL4A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","HTYX10042218","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.0046,0.005,"0.020",0,"TOYOTA: TACOMA 2WD, TACOMA 4WD"]
[2018,"Toyota","JTYXT05.7B6Y","JTYXR0190P32","TOYOTA","TOYOTA TUNDRA 4WD","09-SK3A",0,5.663,5760,7200,6000,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9TYX01085296","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.558,0.59,"1.15",0.035,"LEXUS: LX 570  TOYOTA: LAND CRUISER WAGON 4WD"]
[2018,"Toyota","JTYXT05.7M5W","JTYXR0190P32","TOYOTA","TOYOTA TUNDRA 2WD","05-GSK1",0,3.9560000000000004,4270,5700,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","5TYX01057917","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.02,0.03,"0.20",0.013000000000000001,"TOYOTA: SEQUOIA 2WD, SEQUOIA 4WD, TUNDRA 2WD, TUNDRA 4WD"]
[2018,"Toyota","JTYXV02.0K6B","JTYXR0130P72","TOYOTA","C-HR","18-ZX2C",0,1.987,3300,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","JTYX10044678","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.005,0,"0.05",0,"TOYOTA: C-HR"]
[2018,"Toyota","JTYXV02.5P35","JTYXR0165J72","TOYOTA","CAMRY HYBRID XLE/SE","18-AV3H",0,2.487,3565,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","JTYX10047550","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",1E-3,0,"0.20",0,"TOYOTA: CAMRY HYBRID LE"]
[2018,"Toyota","JTYXV03.5M5A","JTYXR0165P12","LEXUS","GS 200t F SPORT","16-AE1A",0,1.998,3860,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","GTYX10036556","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",1E-3,0.01,"0.20",0.013000000000000001,"LEXUS: GS 350, GS 350 AWD, GS 350 F SPORT, IS 300 AWD, IS 350, IS 350 AWD, RC 300 AWD, RC 350, RC 350 AWD"]
[2018,"Volkswagen Group of","JVGAJ02.0A3A","JVGAR0135ACT","VOLKSWAGEN","Tiguan","UTI017",0,1.984,3885,5247,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","JVGA10048151","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.323,0.323,"0.350",0,"Volkswagen: Tiguan, Tiguan 4Motion"]
[2018,"Volkswagen Group of","JVGAJ03.0AUE","JVGAR0155NAH","AUDI","A8","D3UF-DAQ",0,2.995,4553,null,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","DADX10019950","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Audi: A8, A8L"]
[2018,"Volkswagen Group of","JVGAT02.0AAA","JVGAR0135VCS","VOLKSWAGEN","Atlas","VW416070129",0,3.6,4713,5732,5000,"A","All Wheel Drive","A","Automatic",null,8,"Y","N",null,null,"N","JVGA10046317","MFR","65","Evap Canister Bleed Test","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.015700000000000002,0.016,"0.020",0,"Volkswagen: Atlas"]
[2018,"Volkswagen Group of","JVGAV02.0APA","JVGAR0110ABB","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.26,0.27,"0.35",0.014,"Audi: A3 Cabriolet quattro, A3 quattro, TT Coupe quattro, TT Roadster quattro  Volkswagen: GTI, Golf, Golf Alltrack, Golf SportWagen, Golf SportWagen 4Motion"]
[2018,"Volkswagen Group of","JVGAV02.0VPD","JVGAR0110VBD","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.05",0,"Volkswagen: Jetta"]
[2018,"Volkswagen Group of","JVGAV06.8ELP","JVGAR0220EAP","Bentley","Arnage","10548",0,6.7,5700,6690,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N","6BEX01064616","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.043000000000000003,0.04,"0.20",2E-3,"Bentley: Mulsanne"]
[2018,"Volvo","JVVXJ02.0A70","JVVXR0142EV4","Volvo","XC90 T6 AWD","201712",0,1.969,4669,6060,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HVVX10041637","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.17020000000000002,0.18100000000000002,"0.500",0.0106,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2018,"Volvo","JVVXJ02.0B70","JVVXR0142EV4","Volvo","XC90 T6 AWD","201712",0,1.969,4669,6060,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HVVX10041638","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2054,0.20800000000000002,"0.500",0.0022,"Volvo Cars of North America, LLC: XC90 AWD"]
[2017,"BMW","HBMXT03.0F15","HBMXR0170N63","BMW","750i","CY33005",0,4.4,4641,5788,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000837","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.01,0.02,"0.20",0.008,"BMW: X5 sDrive35i, X5 xDrive35i, X6 sDrive35i, X6 xDrive35i"]
[2017,"BMW","HBMXV01.5I8P","HBMXR0090I8P","BMW","I8","VX64011",0,1.5,3455,4090,3750,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"Y","EBMX10029547","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.009000000000000001,0.01,"0.05",0,"BMW: I8"]
[2017,"BMW","HBMXV02.0B4X","HBMXR0150G30","BMW","530i xDrive","G457602",0,2,3878,4976,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10044989","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.041,0.04,"0.20",0,"BMW: 530i, 530i xDrive"]
[2017,"BMW","HBMXV02.0M48","HBMXR0130F45","Mini","Mini Cooper Countryman","3B62508",0,1.5,3360,4376,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HBMX10043378","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC",0.006,0.01,"0.05",0,"Mini: JOHN COOPER WORKS CLUBMAN ALL4"]
[2017,"BMW","HBMXV03.0B58","HBMXR0130F3X","BMW","330i","5D42601",0,2,3541,4530,3875,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HBMX10042338","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.2523,0.252,"0.300",0,"BMW: 340i, 340i xDrive, 340i xDrive Gran Turismo, 440i Convertible, 440i Coupe, 440i Gran Coupe, 440i xDrive Convertible, 440i xDrive Coupe, 440i xDrive Gran Coupe"]
[2017,"FCA US LLC","HCRXD06.45V0","HCRXF0272TC0","Dodge","RAM 1500 PICKUP 4WD","V3DR10673",0,3.7,4858,6650,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","8CRX01051891","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.4,0.4,"1.00",0,"RAM: 2500 Cab Chassis 4X2, 2500 Cab Chassis 4X4"]
[2017,"FCA US LLC","HCRXD06.45V1","HCRXF0272TC2","Dodge","RAM 3500 CAB CHAS 2WD","K7DC88916",0,5.7,10000,12500,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","9CRX10000425","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.003,0,"0.05",0,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2017,"FCA US LLC","HCRXJ02.45P1","HCRXR0116PK0","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017735","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.41200000000000003,0.41000000000000003,"0.50",0,"Dodge: Dart, Dart GT"]
[2017,"FCA US LLC","HCRXJ02.45PA","HCRXR0118PPB","Dodge","Dart","L4PFD6873",3,2,3257,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10043879","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.008,0.01,"0.05",0,"Jeep: Cherokee 4X4, Cherokee FWD"]
[2017,"FCA US LLC","HCRXJ02.4CP0","HCRXR0118FE1","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017736","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.10600000000000001,0.11,"0.20",0,"Chrysler: 200  Dodge: Dart, Dart GT"]
[2017,"FCA US LLC","HCRXT02.45P3","HCRXR0118PP0","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017736","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.10600000000000001,0.11,"0.20",0,"Jeep: Cherokee 4x4 Active Drive II, Cherokee Trailhawk 4X4"]
[2017,"FCA US LLC","HCRXT03.65P1","HCRXR0140RK0","Dodge","CARAVAN 2WD","K8RTY0076",1,3.3000000000000003,4358,6050,4750,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","8CRX10000277","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Chrysler: Pacifica"]
[2017,"FCA US LLC","HCRXT03.65PB","HCRXR0225RKA","Dodge","Ram 1500 Pickup 4wd","K9DS16774",0,4.7,5489,6800,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX10000194","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2017,"FCA US LLC","HCRXV01.45P1","HCRXR0100PK0","Fiat","500","L2FFF2534",0,1.4000000000000001,2421,3300,2750,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N","CCRX10011975","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.264,0.27,"0.65",0.01,"FIAT: 500"]
[2017,"FCA US LLC","HCRXV03.65PB","HCRXR0141PKA","Chrysler","300 AWD","L5LXF1269",3,3.6,4324,5350,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","HCRX10044798","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.444,0.45,"0.50",0.01,"Chrysler: 300, 300 AWD  Dodge: Charger, Charger AWD"]
[2017,"FOMOCO","HFMXD03.76BG","HFMXR0190NBS","Ford","T350 FFV Van","ETH1-3.7-J-465",0,3.7,6925,9500,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10028137","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.35400000000000004,0.35000000000000003,"1.00",0,"Ford: TRANSIT T150 VAN FFV, TRANSIT T250 VAN 2WD FFV, TRANSIT T250 WAGON 2WD FFV, TRANSIT T350 VAN 2WD FFV, TRANSIT T350 WAGON 2WD FFV"]
[2017,"FOMOCO","HFMXD03.77BX","HFMXF0190NBS","Ford","T350 FFV Van","ETH1-3.7-J-465",0,3.7,6925,9500,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10028135","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.329,0.33,"001.75",0,"Ford: TRANSIT T350 CHASSIS CAB, TRANSIT T350 CUTAWAY"]
[2017,"FOMOCO","HFMXT01.52GA","HFMXR0130NDF","Ford","Transit Connect FWD","GHC1-2.5-C-753",1,2.5,3968,5280,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HFMX10039895","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0,0,"000.05",0,"Ford: ESCAPE AWD, ESCAPE FWD"]
[2017,"FOMOCO","HFMXT02.02HA","HFMXR0130NDF","Ford","Transit Connect FWD","GHC1-2.5-C-753",1,2.5,3968,5280,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HFMX10039897","MFR","23","2-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.1434,0.14300000000000002,"000.400",0,"Ford: ESCAPE AWD, ESCAPE FWD  Lincoln: MKC  AWD, MKC  FWD"]
[2017,"FOMOCO","HFMXT02.52FB","HFMXR0130NDF","Ford","Transit Connect FWD","GHC1-2.5-C-753",1,2.5,3968,5280,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HFMX10039895","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"000.05",0,"Ford: ESCAPE FWD"]
[2017,"FOMOCO","HFMXT03.54HE","HFMXR0265NBC","LINCOLN","NAVIGATOR 4X4 EXT.","9B51-5.4-C-796",0,5.4,6356,7900,6500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","9FMX01085042","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.374,0.37,"000.90",0,"Ford: Expedition 2WD, Expedition 4WD, Expedition EL 2WD, Expedition EL 4WD  Lincoln: Navigator 2WD, Navigator 4WD, Navigator L 2WD, Navigator L 4WD"]
[2017,"FOMOCO","HFMXT03.55HW","HFMXR0190NBD","Ford","T350 FFV Van","ETH1-3.7-J-465",0,3.7,6925,9500,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10028311","MFR","24","Federal fuel refueling test (ORVR)","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","150","OMHCE",0.14200000000000002,0.17,"0.20",0.027,"Ford: Transit T150 Wagon"]
[2017,"FOMOCO","HFMXT05.03DL","HFMXR0235NBC","Ford","F-150 4X4","FFC1-5.0-554",0,5,5260,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10033209","MFR","24","Federal fuel refueling test (ORVR)","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.031,0.04,"0.20",0.01,"Ford: F150 4WD FFV BASE PAYLOAD LT, F150 5.0L 2WD FFV GVWR>7599 LBS, F150 5.0L 4WD FFV GVWR>7599 LBS, F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2017,"FOMOCO","HFMXV02.0VZT","HFMXR0145HCE","Lincoln","MKZ (HEV)","HC91-2.0-J-815",0,2,3919,4910,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","HFMX91003073","EPA","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.15080000000000002,0.151,"0.300",0,"Ford: C-MAX Hybrid FWD, FUSION HYBRID FWD  Lincoln: MKZ HYBRID FWD"]
[2017,"FOMOCO","HFMXV02.7VLM","HFMXR0130NDE","Ford","MKZ","HC91-2.0-J-813",1,2,3951,4960,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HFMX10040098","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","OMHCE",0.2071,0.20700000000000002,"0.300",0,"Ford: FUSION AWD"]
[2017,"FOMOCO","HFMXV03.5VGT","HFMXR0125NAA","Ford","GT","HS105006",0,3.5,3352,3700,3625,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"Y","N",null,null,"N","HFMX10044598","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.367,0.41000000000000003,"0.50",0.043000000000000003,"Ford: Ford GT"]
[2017,"GM","HGMXD06.0394","HGMXF0223850","CHEVROLET","K35 CHEV CAB CHASSIS 4WD","60XEKCB966",0,6,11300,13200,12000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","GGMX10037051","MFR","15","Spitback","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","SPITBACK",0.67,0.7000000000000001,"1.0",0,"Chevrolet: C25 SILVERADO 2WD, C35 SILVERADO 2WD, K25 SILVERADO 4WD, K35 SILVERADO 4WD  GMC: C25 SIERRA 2WD, C35 SIERRA 2WD, K25 SIERRA 4WD, K35 SIERRA 4WD"]
[2017,"GM","HGMXD06.0399","HGMXR0223842","CHEVROLET","CK15903","43KP9107",15,6,6867,11400,9000,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AGMX01047754","MFR","15","Spitback","6","EPA Unleaded Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","SPITBACK",0.01,0,"1.0",0,"Chevrolet: C35 SILVERADO 2WD, K35 SILVERADO 4WD  GMC: C35 SIERRA 2WD, K35 SIERRA 4WD"]
[2017,"GM","HGMXJ02.4199","HGMXR0133703","GMC","TERRAIN AWD","24TALN2506",0,2.4,4109,null,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","BGMX10010512","MFR","32","Federal Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2017,"GM","HGMXJ03.6165","HGMXR0112835","CHEVROLET","1ND69","2215NP4000",1,2,3339,4240,3625,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061625","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.58,0.58,"0.65",0,"Cadillac: CT6 AWD"]
[2017,"GM","HGMXT02.5200","HGMXR013835A","GMC","CANYON 4WD","25SPHN1023",0,2.5,4194,5600,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040906","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: COLORADO 2WD, COLORADO 4WD  GMC: CANYON 2WD, CANYON 4WD"]
[2017,"GM","HGMXT03.6161","HGMXR013835A","GMC","CANYON 4WD","25SPHN1023",0,2.5,4194,5600,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040906","MFR","32","Federal Fuel Running Loss","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"Chevrolet: COLORADO 2WD, COLORADO 4WD  GMC: CANYON 2WD, CANYON 4WD"]
[2017,"GM","HGMXT05.3384","HGMXR016150A","GMC","C15 SIERRA 2WD","43CPHN1208",0,4.3,4839,6500,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","HGMX10040901","MFR","34","Federal fuel 3-day evap","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.383,0.383,"0.500",0,"Chevrolet: C15 SILVERADO 2WD, C1500 TAHOE 2WD, K15 SILVERADO 4WD, K1500 TAHOE 4WD  GMC: C15 SIERRA 2WD, C1500 YUKON 2WD, K15 SIERRA 4WD, K1500 YUKON 4WD"]
[2017,"GM","HGMXT06.2374","HGMXR0223840","CHEVROLET","CC10903","53XECP8101",0,5.3,5950,7300,6000,"A","All Wheel Drive","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX10002177","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"0.05",0,"Cadillac: ESCALADE 2WD, ESCALADE 4WD  GMC: C1500 YUKON XL 2WD, K1500 YUKON XL 4WD"]
[2017,"GM","HGMXV01.4099","HGMXR0095805","BUICK","ENCORE AWD","143SV855DA",0,1.4000000000000001,3344,null,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic","T6",6,"Y","N",null,null,"N","GGMX10039070","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.545,0.54,"0.65",0,"Buick: ENCORE, ENCORE AWD  Chevrolet: SONIC, SONIC 5, TRAX, TRAX AWD"]
[2017,"GM","HGMXV02.0021","HGMXR0133810","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017013","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.20500000000000002,0.2,"0.50",0,"Buick: REGAL, REGAL AWD"]
[2017,"GM","HGMXV02.0050","HGMXR0116832","CADILLAC","CT6 HYBRID","20YS16PV68",0,2,4526,null,4750,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y","HGMX10046088","MFR","24","Federal fuel refueling test (ORVR)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.008,0.01,"0.20",0,"Cadillac: CT6 HYBRID"]
[2017,"GM","HGMXV02.5001","HGMXR0133810","CHEVROLET","1WB19","3516WN4002",1,3.5,3579,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01062380","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.253,0.25,"0.50",0,"Chevrolet: IMPALA"]
[2017,"GM","HGMXV06.2088","HGMXR0133880","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017012","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28800000000000003,0.29,"0.65",0,"Chevrolet: SS"]
[2017,"GM","HGMXV06.2090","HGMXR0133810","BUICK","4HP69","3846HN4008",13,3.9,3824,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01062010","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.011000000000000001,0.01,"0.20",0,"Chevrolet: CORVETTE"]
[2017,"Honda","HHNXV01.56H3","HHNXR0113VSB","HONDA","CIVIC 4DR SEDAN 1.5L","EGAA4C",0,1.5,2908,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10037926","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",6.3E-3,0.006,"0.020",null,"Honda: CIVIC 2Dr, CIVIC 4Dr"]
[2017,"Honda","HHNXV01.8FA3","HHNXR0106VFB","HONDA","HR-V 4WD","EG1M2C",0,1.8,3119,null,3375,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N","GHNX10033641","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.026000000000000002,0.03,"0.20",null,"Honda: HR-V AWD, HR-V FWD"]
[2017,"Honda","HHNXV02.4TA3","HHNXR0121VFA","ACURA","TLX","EFJ24A",0,3.5,3789,null,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","FHNX10031142","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.023,0.03,"0.20",0.01,"Acura: TLX FWD"]
[2017,"Honda","HHNXV03.5KH4","HHNXR0129VFA","ACURA","NSX","DH8G1D",0,3.5,3944,4497,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,9,"Y","N",null,null,"Y","HHNX10039957","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Acura: NSX"]
[2017,"Honda","HHNXV03.5VH3","HHNXR0151VFA","ACURA","MDX 4WD","EEJ63A",0,3.5,4575,null,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","EHNX10024101","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Acura: MDX AWD, MDX FWD  Honda: PILOT AWD, PILOT FWD"]
[2017,"Hyundai","HHYXV02.01E5","HHYXR01301EG","Hyundai","Elantra","AD7N0GS47C1",0,2,2912,3924,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HHYX10038652","MFR","67","Leak Test - Port Near Canister","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","LEAK-DIA",0,0,"0.020",0,"HYUNDAI MOTOR COMPANY: Elantra, Elantra SE"]
[2017,"Hyundai","HHYXV02.41W5","HHYXR0130AVE","Hyundai","Santa Fe Sport","AN3F0HU17A1",0,2,3878,5181,4250,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","DHYX10019914","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.393,0.39,"0.50",0,"HYUNDAI MOTOR COMPANY: Santa Fe Sport AWD, Santa Fe Sport FWD"]
[2017,"Hyundai","HHYXV03.31LF","HHYXR01391LE","HYUNDAI","AZERA","HG2L3AU11B2",0,3.3000000000000003,3775,4785,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","CHYX10016163","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.29400000000000004,0.29,"0.50",0,"HYUNDAI MOTOR COMPANY: Azera, Azera Limited"]
[2017,"Jaguar Land Rover L","HJLXJ03.0FSP","HJLXR0140P1Z","Land Rover","Range Rover Evoque","3EVPP037",0,2,3995,5181,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","EJLX10028183","MFR","24","Federal fuel refueling test (ORVR)","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC",0.009000000000000001,0.01,"0.20",0,"Jaguar: F-Pace"]
[2017,"Kia","HKMXT02.44NP","HKMXR0140DNG","HYUNDAI","Tucson","TL6N0HU03AC",0,2,3489,4740,3750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GHYX10034918","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.1709,0.171,"0.300",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FE AWD, Sportage FE FWD, Sportage FWD"]
[2017,"Kia","HKMXV01.6DDF","HKMXR01284DE","KIA","Forte5","YD3R6AU09A1",0,1.6,3025,4056,3375,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10025127","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.40700000000000003,0.41000000000000003,"0.65",0,"KIA MOTORS CORPORATION: Forte Koup, Forte5"]
[2017,"Kia","HKMXV02.04E5","HKMXR01284EE","KIA","Forte ECO","YD3N8GF23A1",0,1.8,2820,3880,3125,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10023376","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.323,0.32,"0.50",0,"KIA MOTORS CORPORATION: Forte"]
[2017,"Kia","HKMXV02.04FP","HKMXR01344FG","Kia","Forte","YD7N0AU13AC",0,2,2928,3902,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","HKMX10039694","MFR","68","Leak Test - Port Near Fuel Pipe","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","LEAK-DIA",1E-3,1E-3,"0.020",0,"KIA MOTORS CORPORATION: Forte"]
[2017,"Maserati","HMAXV03.8DFI","HMAXR0110161","MASERATI","QUATTROPORTE GTS","070989",1,3.8000000000000003,4495,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","HMAX10042289","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",2E-3,0.01,"0.20",0.01,"MASERATI: QUATTROPORTE GTS"]
[2017,"MAZDA","HTKXV02.0CDA","HTKXR0115GCP","MAZDA","MAZDA3","5ECPES1-004",0,2,2919,4001,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FTKX10030647","MFR","38","CA fuel 3-day evap.","46","CARB LEV3 E10 Regular Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.21150000000000002,0.21200000000000002,"0.300",0,"MAZDA: MAZDA3 4-Door, MAZDA3 5-Door"]
[2017,"MAZDA","HTKXV02.5FBA","HTKXR0111GAK","MAZDA","MAZDA6","4EFPY31-004",2,2.5,3183,4226,3500,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N","ETKX10022981","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.008,0.01,"0.20",0.004,"MAZDA: MAZDA3 4-Door, MAZDA3 5-Door"]
[2017,"Mercedes-Benz","HMBXJ06.0U2A","HMBXR0170LNS","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10035378","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2048,0.24,"0.275",0.035,"Mercedes-Benz: AMG S 65, Maybach S 600, Maybach S 650 (convertible), S 600, S 65 AMG (convertible), S 65 AMG (coupe)"]
[2017,"Mercedes-Benz","HMBXT03.5U2B","HMBXR0170LND","Mercedes-Benz","ML 350 4MATIC","W166E35DEH-Z2036",1,3.498,4813,6283,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","CMBX10018716","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.008,0.01,"0.05",0,"Mercedes-Benz: GLE 350 4MATIC"]
[2017,"Mercedes-Benz","HMBXV03.0U2A","HMBXR0160LNF","Mercedes-Benz","E 350 4 MATIC","W212E35DEH-Z2004-6",0,3.498,4255,5225,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","DMBX10020917","MFR","24","Federal fuel refueling test (ORVR)","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.024,0.03,"0.20",0.004,"Mercedes-Benz: E 400 (convertible), E 400 (coupe), E 400 4MATIC (coupe)"]
[2017,"Mercedes-Benz","HMBXV05.5U2A","HMBXR0170LNS","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10035378","MFR","38","CA fuel 3-day evap.","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2048,0.24,"0.275",0.035,"Mercedes-Benz: AMG S 63 4MATIC, AMG S 63 4MATIC (convertible), AMG S 63 4MATIC (coupe), S 550, S 550 (convertible), S 550 4MATIC, S 550 4MATIC (W), S 550 4MATIC (coupe), S 550 4MATIC Maybach"]
[2017,"Nissan","HNSXD05.6V9B","HNSXF0174PBB","NISSAN","NISSAN NV3500 M S/R","TYB016",0,5.6000000000000005,6187,9900,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","CNSX10011388","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.48800000000000004,0.49,"1.00",0,"NISSAN: NV2500 Cargo Van, NV3500 Cargo Van, NV3500 Passenger Van, TITAN XD 2WD, TITAN XD 4WD"]
[2017,"Nissan","HNSXT02.5NFA","HNSXR0123PBA","INFINITI","INFINITI QX60 AWD","GLB066",0,2.5,4665,6000,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y","ENSX10025979","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28200000000000003,0.28,"0.85",0,"INFINITI: QX60 AWD Hybrid, QX60 FWD Hybrid  NISSAN: PATHFINDER Hybrid 2WD, PATHFINDER Hybrid 4WD"]
[2017,"Nissan","HNSXT03.5P7A","HNSXR0120PBC","NISSAN","PATHFINDER 4WD PLATINUM","GKB390",1,3.5,4672,5986,5000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","HNSX10041568","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"INFINITI: QX60 AWD, QX60 FWD  NISSAN: PATHFINDER 2WD, PATHFINDER 4WD"]
[2017,"Nissan","HNSXV01.8M1A","HNSXR0090PBA","NISSAN","NISSAN SENTRA SL","KPB088",0,1.8,2869,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","DNSX10020428","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.203,0.2,"0.50",0,"NISSAN: SENTRA"]
[2017,"Nissan","HNSXV02.0NJA","HNSXR0159MBA","INFINITI","INFINITI Q50 AWD PREMIUM","HRB818",2,2,3850,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N","GNSX10038514","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.025,0.02,"0.20",0,"INFINITI: Q50, Q50 AWD, Q50S, Q50S AWD, Q60, Q60 AWD"]
[2017,"Nissan","HNSXV03.5P7C","HNSXR0120PBA","NISSAN","NISSAN MURANO AWD  SL","JJB066",1,3.5,4041,null,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","FNSX10032244","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.269,0.27,"0.65",0,"NISSAN: MURANO AWD, MURANO FWD"]
[2017,"Pagani S.p.A.","HPGNV06.0ABC","HPGNR0220AA1","Pagani Automobili","PT4","EDV14PAG01",1,6,3197,null,3500,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"N","EPGN10028729","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.13,0.2,"0.2",0.02,"Pagani Automobili S.p.A.: Huayra"]
[2017,"Porsche","HPRXT03.6MCS","HPRXR0230RED","Porsche","Cayenne S","EC-92AIIS-15",0,3.6,5005,6305,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FPRX10033050","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.5770000000000001,0.6,"0.65",0.024,"Porsche: Cayenne GTS, Cayenne S"]
[2017,"Roush","HRIIV05.0VKM","HRIIR0125NDA","Ford","Mustang","FZG1-5.0-F-560",0,5,3941,4250,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FFMX10031989","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.219,0.22,"0.50",0,"Roush Industries, Inc.: Roush Stage 3 Mustang"]
[2017,"Subaru","HFJXJ02.5HRV","HFJXR01485DX","SUBARU","OUTBACK","FBV-VC16",0,2.5,3666,null,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","FFJX10040549","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.011600000000000001,0.012,"0.020",0,"Subaru: LEGACY, OUTBACK"]
[2017,"Subaru","HFJXV02.0AJM","HFJXR01223AU","SUBARU","BRZ","DBV-MP42",1,2,2822,null,3125,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DFJX10017437","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.005,0.01,"0.20",0.004,"Subaru: BRZ  TOYOTA: 86"]
[2017,"Toyota","HTYXT03.5M5M","HTYXR0165P82","TOYOTA","SIENNA AWD","17-GL4A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","HTYX10042218","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.0046,0.005,"0.020",0,"LEXUS: RX 350, RX 350 AWD  TOYOTA: HIGHLANDER, HIGHLANDER AWD, HIGHLANDER AWD LE, HIGHLANDER LE/XLE/SE/LTD, SIENNA, SIENNA AWD"]
[2017,"Toyota","HTYXT04.6B6X","HTYXR0190P32","TOYOTA","TOYOTA TUNDRA 4WD","09-SK3A",0,5.663,5760,7200,6000,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9TYX10000283","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.008,0.01,"0.05",0,"LEXUS: GX 460"]
[2017,"Toyota","HTYXV01.5B6B","HTYXR0085P12","SCION","iQ","11-NJ2C",0,1.329,2135,null,2375,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N","SF","Single Fuel","N","BTYX10009641","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",1E-3,0,"0.05",0,"TOYOTA: YARIS"]
[2017,"Toyota","HTYXV01.8M5B","HTYXR0115P12","SCION","tC","11-AT1M",0,2.494,3110,null,3375,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N","SF","Single Fuel","N","BTYX10009496","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","150","HC",1E-3,0.01,"0.20",0.013000000000000001,"TOYOTA: COROLLA LE ECO, COROLLA iM"]
[2017,"Toyota","HTYXV03.5M5A","HTYXR0165P12","LEXUS","GS 200t F SPORT","16-AE1A",0,1.998,3860,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","GTYX10036556","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",1E-3,0.01,"0.20",0.013000000000000001,"LEXUS: GS 350, GS 350 AWD, GS 350 F SPORT"]
[2017,"Volkswagen Group of","HVGAJ02.0AAC","HVGAR0155AAM","AUDI","Q7","HAUT-Q7A",0,3,5022,6479,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HVGA10038867","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.7250000000000001,0.7250000000000001,"0.900",0,"Audi: Q7"]
[2017,"Volkswagen Group of","HVGAJ02.0VUE","HVGAR0125VAT","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX01080443","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.41000000000000003,0.4,"0.5",0,"Volkswagen: Tiguan, Tiguan 4Motion, Tiguan Limited, Tiguan Limited 4Motion"]
[2017,"Volkswagen Group of","HVGAT06.0EAR","HVGAR0155ECR","AUDI","Q7","HAUT-Q7A",0,3,5022,6479,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","HVGA91002993","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.35450000000000004,0.35400000000000004,"1.150",0,"Bentley: Bentayga"]
[2017,"Volkswagen Group of","HVGAV02.0AUB","HVGAR0140AAC","AUDI","S5","8365-BMQ",0,4.163,3891,null,4250,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N","SF","Single Fuel","N","8ADX01078802","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.01,0,"0.2",1E-3,"Audi: A5 Cabriolet, A5 quattro"]
[2017,"Volkswagen Group of","HVGAV02.0VPE","HVGAR0125VBD","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX91000391","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.193,0.23,"0.35",0.041,"Volkswagen: CC"]
[2017,"Volkswagen Group of","HVGAV06.5LLR","HVGAR0130NAJ","AUDI","R8","8375-RAQ",1,4.163,3671,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01076741","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.4,0.4,"0.5",0.017,"Lamborghini: Aventador Coupe, Aventador Coupe LP740-4, Aventador Roadster, Aventador Roadster LP740-4"]
[2017,"Volvo","HVVXV02.0L3T","HVVXR0130EV2","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003726","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.339,0.339,"0.500",0,"Volvo Cars of North America, LLC: S60 Polestar AWD, V60 Polestar AWD"]
[2016,"BMW","GBMXJ03.0N55","GBMXR0130N54","BMW","335i xDrive","KS33736",0,3,3825,4883,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000612","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.012,0.01,"0.05",2E-3,"BMW: 335i xDrive Gran Turismo, 435i Convertible, 435i Coupe, 435i Gran Coupe, 435i xDrive Convertible, 435i xDrive Coupe, 435i xDrive Gran Coupe, M2, M235i, M235i Convertible, M235i xDrive, M235i xDrive Convertible, X3 xDrive35i, X4 M40i, X4 xDrive35i"]
[2016,"BMW","GBMXV01.5M36","GBMXR0100F5X","Mini","Mini Cooper (5-doors)","T826907",0,1.5,2815,3750,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FBMX10033892","MFR","65","Evap Canister Bleed Test","47","CARB LEV3 E10 Premium Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",8.6E-3,0.009000000000000001,"0.020",0,"Mini: MINI COOPER HARDTOP 2 DOOR, MINI COOPER HARDTOP 4 DOOR, Mini Cooper Convertible"]
[2016,"BMW","GBMXV02.0B46","GBMXR0130F45","BMW","X1 xDrive28i","P880003",0,2,3660,4720,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","GBMX10037255","MFR","65","Evap Canister Bleed Test","46","CARB LEV3 E10 Regular Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0.019700000000000002,0.02,"0.020",0,"BMW: X1 sDrive28i, X1 xDrive28i"]
[2016,"BMW","GBMXV03.0S55","GBMXR0130N54","BMW","335i xDrive","KS33736",0,3,3825,4883,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX01071518","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.005,0,"0.20",0,"BMW: M3, M4 Convertible, M4 Coupe, M4 GTS"]
[2016,"FCA US LLC","GCRXD03.65V1","GCRXR0190TC1","RAM","Promaster 3500","L4VF11444",0,3.6,5066,9350,7000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10025964","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.508,0.51,"1.75",0,"RAM: Promaster 2500 Cab Chassis, Promaster 3500 Cab Chassis"]
[2016,"FCA US LLC","GCRXD06.45W1","GCRXF0205TC0","Dodge","RAM 3500 CAB CHAS 2WD","K7DC88916",0,5.7,10000,12500,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","9CRX01070371","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.754,0.76,"1.25",0.01,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2016,"FCA US LLC","GCRXJ02.45P4","GCRXR0116PK1","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017735","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.41200000000000003,0.41000000000000003,"0.65",0,"FIAT: 500X, 500X AWD  Jeep: Cherokee 4X4, Cherokee FWD, Renegade 4x4"]
[2016,"FCA US LLC","GCRXJ02.45PA","GCRXR0116PKA","Dodge","Dart","L2PFD3317",0,2,3260,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","DCRX10022230","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"0.05",0,"Chrysler: 200  Dodge: Dart"]
[2016,"FCA US LLC","GCRXJ03.65PA","GCRXR0150RKA","Chrysler","TOWN & COUNTRY FWD","K8RTY0076",3,3.3000000000000003,4457,6050,4750,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01077407","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.47700000000000004,0.48,"0.90",0,"Chrysler: Town & Country  Dodge: Grand Caravan"]
[2016,"FCA US LLC","GCRXT02.45P1","GCRXR0116PK1","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017736","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.10600000000000001,0.11,"0.20",0,"Jeep: Cherokee 4x4 Active Drive II, Cherokee Trailhawk 4X4"]
[2016,"FCA US LLC","GCRXT03.65PD","GCRXR0225RKA","Dodge","Ram 1500 Pickup 4wd","K9DS16774",0,4.7,5489,6800,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX10000196","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"0.05",0,"RAM: 1500 4X2, 1500 4X4"]
[2016,"FCA US LLC","GCRXT05.75P1","GCRXR0190RK0","Dodge","Ram 1500 Pickup 4wd","K9DS16740",0,4.7,5489,6800,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01086058","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.667,0.68,"1.15",0.01,"RAM: 1500 4X2, 1500 4X4"]
[2016,"FCA US LLC","GCRXV02.45P3","GCRXR0116PK0","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX91001210","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.332,0.34,"0.65",0.01,"Dodge: Dart, Dart GT"]
[2016,"Ferrari","GFEXV03.9TUR","GFEXR0175149","Ferrari","458 Italia Spyder","ZFF67NHB000171765",0,4.5,3495,4046,3875,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","AFEX10008693","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.014,0.01,"0.05",0,"Ferrari North America, Inc.: 488 GTB, 488 Spider, California T"]
[2016,"FOMOCO","GFMXD06.27HV","GFMXF0265NAS","Ford","F350 Incomplete 4x4","BFA1-6.2-J-006",0,6.2,10603,12600,11000,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","BFMX10006406","MFR","15","Spitback","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","SPITBACK",0.46,0.5,"001.0",0,"Ford: F350 INCOMPLETE 2WD FFV, F350 INCOMPLETE 4WD FFV"]
[2016,"FOMOCO","GFMXT02.32ED","GFMXR0125NBV","Ford","Escape AWD","DM21-1.6-F-223",0,1.6,3714,4770,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DFMX91001260","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.215,0.26,"000.65",0.043000000000000003,"Lincoln: MKC  AWD"]
[2016,"FOMOCO","GFMXT02.72GH","GFMXR0135NBB","Lincoln","MKX AWD","GD91-3.7-J-719",0,3.7,4535,5620,4750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","GFMX10034916","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.317,0.36,"0.65",0.043000000000000003,"Lincoln: MKX AWD, MKX FWD"]
[2016,"FOMOCO","GFMXT02.73JJ","GFMXR0160ABC","Ford","F-150 Super Cab Max","FFC1-2.7-F-545",0,2.7,4932,7000,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FFMX91002409","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.658,0.66,"1.15",0,"Ford: F-150 2WD PAYLOAD GVWR 6650 LBS., F150 4WD PAYLOAD GVWR 6800 LBS., F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2016,"FOMOCO","GFMXV01.5VDG","GFMXR0125NBV","Ford","Fusion FWD","EC73-1.5-F-475",0,1.5,3468,3750,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","EFMX10025089","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.044000000000000004,0.04,"000.20",0,"Ford: FUSION FWD"]
[2016,"FOMOCO","GFMXV02.0VEM","GFMXR0125NBV","Ford","MKZ AWD","DC93-2.0-C-403",0,2,3940,4250,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DFMX10020690","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.31,0.35000000000000003,"000.50",0.043000000000000003,"Ford: FUSION AWD, FUSION FWD  Lincoln: MKZ AWD, MKZ FWD"]
[2016,"FOMOCO","GFMXV03.5VEP","GFMXR0145GBV","FORD","FLEX","AP33-3.5-J-566",0,3.5,4964,6250,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","AFMX10002633","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",1E-3,0,"000.05",0,"Ford: EXPLORER AWD, FLEX AWD, Interceptor Sedan AWD, Police Interceptor Utility AWD, TAURUS AWD  Lincoln: MKS AWD, MKT AWD"]
[2016,"FOMOCO","GFMXV03.7VHJ","GFMXR0145GBV","FORD","FREESTYLE AWD","8P51-3.5-F-509",4,3.5,4431,5460,4750,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","AFMX10001952","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"000.05",0,"Lincoln: MKT HEARSE AWD, MKT LIMO AWD"]
[2016,"GM","GGMXD06.0395","GGMXR0223841","GMC","CC15903","43XECP6053",6,4.8,5727,9600,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01068129","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.7070000000000001,0.71,"1.00",0,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD PASS  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD PASS"]
[2016,"GM","GGMXD06.0399","GGMXR0223842","GMC","CC15903","43XECP6053",6,4.8,5727,9600,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX10001567","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0,0,"0.05",0,"Chevrolet: C35 SILVERADO 2WD, K35 SILVERADO 4WD  GMC: C35 SIERRA 2WD, K35 SIERRA 4WD"]
[2016,"GM","GGMXJ02.4199","GGMXR0138813","GMC","TERRAIN AWD","30TALP5135",1,3,4197,5300,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BGMX10008883","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.263,0.26,"0.65",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2016,"GM","GGMXT02.4151","GGMXR0138813","GMC","TERRAIN AWD","30TALP5135",1,3,4197,5300,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BGMX10008883","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.263,0.26,"0.65",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN FWD"]
[2016,"GM","GGMXT03.6161","GGMXR0138813","GMC","TERRAIN AWD","30TALP5135",1,3,4197,5300,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BGMX10008882","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"0.05",0,"Chevrolet: COLORADO 2WD, COLORADO 4WD  GMC: CANYON 2WD, CANYON 4WD"]
[2016,"GM","GGMXT04.3187","GGMXR0223840","CHEVROLET","CC10903","53XECP8101",0,5.3,5950,7300,6000,"A","All Wheel Drive","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01075227","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.7120000000000001,0.71,"0.90",0,"Chevrolet: C15 SILVERADO 2WD, K15 SILVERADO 4WD  GMC: C15 SIERRA 2WD, K15 SIERRA 4WD"]
[2016,"GM","GGMXT05.3384","GGMXR0223840","GMC","CC15903","43XECP6053",6,4.8,5727,9600,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01068130","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.029,0.03,"0.20",0,"Chevrolet: C15 SILVERADO 2WD, C15 SILVERADO 2WD CAB CHASSIS, C1500 SUBURBAN 2WD, K15 SILVERADO 4WD, K15 SILVERADO 4WD CAB CHASSIS, K1500 SUBURBAN 4WD  GMC: C15 SIERRA 2WD, C15 SIERRA 2WD CAB CHASSIS, C1500 YUKON XL 2WD, K15 SIERRA 4WD, K15 SIERRA 4WD CAB CHASSIS, K1500 YUKON XL 4WD"]
[2016,"GM","GGMXV01.4050","GGMXR0095805","SATURN","ZAT48","18X360P101",1,1.8,2962,null,3250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX10002209","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Chevrolet: SPARK"]
[2016,"GM","GGMXV01.4050","GGMXR0095805","SATURN","ZAT48","18X360P101",1,1.8,2962,null,3250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX10002211","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.366,0.37,"0.65",0,"Chevrolet: SPARK"]
[2016,"GM","GGMXV01.8031","GGMXR0095700","SATURN","ZAT48","1888AP8000",0,1.8,2962,null,3250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01079875","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.007,0.01,"0.20",0,"Chevrolet: SONIC, SONIC 5"]
[2016,"GM","GGMXV02.0021","GGMXR0133810","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017014","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Buick: REGAL, REGAL AWD"]
[2016,"GM","GGMXV03.6042","GGMXR0112835","CHEVROLET","1ND69","2215NP4000",1,2,3339,4240,3625,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061625","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.58,0.58,"0.65",0,"Cadillac: CT6 AWD"]
[2016,"GM","GGMXV03.6048","GGMXR0123702","CHEVROLET","2WS69","3825WN4008",31,3.5,3629,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061187","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.217,0.26,"0.50",0.04,"Buick: LACROSSE  Cadillac: XTS  Chevrolet: IMPALA"]
[2016,"GM","GGMXV06.2088","GGMXR0133880","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017013","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.20500000000000002,0.2,"0.50",0,"Chevrolet: SS"]
[2016,"Honda","GHNXJ02.41A3","GHNXR01351FB","ACURA","RDX 4WD","ED8A3A",0,3.5,3901,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DHNX10018366","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.012,0.01,"0.20",0,"Honda: CR-V 2WD, CR-V 4WD"]
[2016,"Honda","GHNXV01.56K2","GHNXR0113VSB","HONDA","CIVIC 4DR SEDAN 1.5L","EGAA4C",0,1.5,2908,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","GHNX10037941","MFR","27","California fuel 2-day evap","46","CARB LEV3 E10 Regular Gasoline","C","AGED","Aged components installed In the emission data vehicle","FA","Federal","T3","Federal Tier 3 Evap","150","HC-TOTAL-EQUIV",0.2179,0.218,"0.300",null,"Honda: CIVIC 2Dr, CIVIC 4Dr"]
[2016,"Honda","GHNXV03.5FH3","GHNXR0121VFB","HONDA","ACCORD","EDA01C",0,2.4,3342,null,3625,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N","DHNX10021284","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.01,0.02,"0.20",0.01,"Honda: ACCORD"]
[2016,"Honda","GHNXV03.5RA3","GHNXR0121VFA","ACURA","TLX","EFJ24A",0,3.5,3789,null,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","FHNX10031137","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.339,0.38,"0.50",0.04,"Acura: TLX 2WD, TLX 4WD"]
[2016,"Hyundai","GHYXV01.81DE","GHYXR01051DE","HYUNDAI","ELANTRA","MD1N8GF29A1",0,1.8,2701,3792,3000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","BHYX10010816","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.019,0.02,"0.05",0,"HYUNDAI MOTOR COMPANY: Elantra, Elantra Limited"]
[2016,"Hyundai","GHYXV03.81NE","GHYXR01401NE","HYUNDAI","GENESIS COUPE","BK3L8AU33B2",0,3.8000000000000003,3576,4409,3875,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","DHYX10017037","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.015000000000000001,0.02,"0.20",0,"HYUNDAI MOTOR COMPANY: Genesis Coupe"]
[2016,"Jaguar Land Rover L","GJLXT05.0002","GJLXR0175001","LAND ROVER","LR4","SDV18",0,4.4,5649,6807,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","EJLX10024511","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.451,0.48,"0.90",0.028,"Land Rover: Range Rover, Range Rover LWB, Range Rover Sport"]
[2016,"Kia","GKMXV01.6DBE","GKMXR01281BE","HYUNDAI","Veloster","FS1R6AU24A1",1,1.6,2736,3748,3000,"F","2-Wheel Drive, Front","AM","Automated Manual","Dual Clutch",6,"Y","N","SF","Single Fuel","N","CHYX91001012","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.405,0.4,"0.65",0,"HYUNDAI MOTOR COMPANY: Veloster"]
[2016,"Kia","GKMXV02.04WE","GKMXR0135DWE","Kia","Sorento","UM5F0U09AC",0,2,4169,5247,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GKMX10032901","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.36100000000000004,0.36,"0.50",0,"KIA MOTORS CORPORATION: Sorento AWD, Sorento FWD"]
[2016,"Kia","GKMXV03.34RE","GKMXR01354RE","Kia","Sorento","UM5L3U01AC",0,3.3000000000000003,4317,5622,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GKMX10032750","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.025,0.02,"0.05",0,"KIA MOTORS CORPORATION: Sorento AWD, Sorento AWD FE, Sorento FWD"]
[2016,"Maserati","GMAXV04.7LEV","GMAXR0198138","MASERATI","QUATTROPORTE","ZAMCD39B000010379",0,4.2,4376,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"N","N","SF","Single Fuel","N","AMAX10005370","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.015000000000000001,0.02,"0.05",0,"MASERATI: GRANTURISMO, GRANTURISMO CONVERTIBLE, QUATTROPORTE"]
[2016,"MAZDA","GTKXV02.55NM","GTKXR0107GBK","MAZDA","CX-3","6ECPES1-023",1,2,2809,3840,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","GTKX10034668","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"MAZDA: CX-3 2WD, CX-3 4WD"]
[2016,"Mercedes-Benz","GMBXJ06.0U2A","GMBXR0170LNF","Mercedes-Benz","ML 350 4MATIC","W166E35DEH-Z2036",1,3.498,4813,6283,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","CMBX10018714","MFR","24","Federal fuel refueling test (ORVR)","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.056,0.06,"0.20",0,"Mercedes-Benz: AMG G65"]
[2016,"Mercedes-Benz","GMBXV00.9U2A","GMBXR0090LNC","Mercedes-Benz","smart fortwo (coupe)","C453E09TC-Z6001",0,0.898,2251,2749,2625,"R","2-Wheel Drive, Rear","M","Manual",null,5,"N","N",null,null,"N","GMBX10037478","MFR","24","Federal fuel refueling test (ORVR)","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.18,0.18,"0.20",0,"Mercedes-Benz: Smart fortwo (COUPE)"]
[2016,"Mercedes-Benz","GMBXV03.0U2A","GMBXR0155LNC","Mercedes-Benz","C 300 4MATIC","Z5023",0,1.991,3715,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","FMBX10037448","MFR","37","California Fuel Running Loss","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL-EQUIV",0,0,"0.05",0,"Mercedes-Benz: C 450 AMG"]
[2016,"Mitsubishi Motors Co","GMTXT03.0G5P","GMTXR0135A1D","MITSUBISHI","LANCER","EB08-CA32",0,1.998,2922,4079,3250,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N","AMTX10003925","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.14,0.14,"0.850",0,"Mitsubishi Motors Corporation: OUTLANDER 4WD"]
[2016,"Nissan","GNSXD05.6Y9A","GNSXF0174PBA","NISSAN","NISSAN NV3500 M S/R","TYB016",0,5.6000000000000005,6187,9900,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","CNSX10011383","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","HD-2D","Federal Heavy-Duty 2-Day Evap (1.75 grams)","120","HC-TOTAL",0.627,0.63,"1.75",0,"NISSAN: NV2500 Cargo Van, NV3500 Cargo Van, NV3500 Passenger Van"]
[2016,"Nissan","GNSXT03.5G7A","GNSXR0120PBB","INFINITI","INFINITI JX35 AWD","GJB181",0,3.5,4497,5937,4750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","DNSX10017322","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.381,0.38,"0.65",0,"INFINITI: QX60 AWD, QX60 FWD  NISSAN: PATHFINDER 2WD, PATHFINDER 4WD, QUEST"]
[2016,"Nissan","GNSXT05.6G9A","GNSXR0174PBA","INFINITI","INFINITI QX56 4WD","TWB022",0,5.6000000000000005,5878,7500,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,7,"Y","N","SF","Single Fuel","N","BNSX10007813","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.41000000000000003,0.41000000000000003,"1.15",0,"INFINITI: QX80 2WD"]
[2016,"Nissan","GNSXV01.6GDA","GNSXR0090PBB","NISSAN","NISSAN JUKE AWD SL","KHEH11",0,1.6,3234,null,3500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","FNSX10032169","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.306,0.31,"0.65",0,"NISSAN: JUKE, JUKE AWD"]
[2016,"Nissan","GNSXV03.5G7C","GNSXR0120PBB","NISSAN","NISSAN MURANO AWD  SL","JJB066",2,3.5,4041,null,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","FNSX10032249","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.08700000000000001,0.09,"0.20",0,"NISSAN: MURANO AWD, MURANO FWD"]
[2016,"Nissan","GNSXV03.7GAB","GNSXR0149MBB","INFINITI","INFINITI EX35 AWD JOURNEY","LTB069",0,3.5,4008,null,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,5,"Y","N","SF","Single Fuel","N","8NSX01078010","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.433,0.43,"0.50",0,"INFINITI: QX50, QX50 AWD"]
[2016,"Porsche","GPRXT04.8CTD","GPRXR0230RED","Porsche","Cayenne S","EC-92AIIS-15",0,3.6,5005,6305,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FPRX10033049","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.8200000000000001,0.84,"1.15",0.024,"Porsche: Cayenne Turbo, Cayenne Turbo S"]
[2016,"Porsche","GPRXT04.8CTD","GPRXR0230RED","Porsche","Cayenne S","EC-92AIIS-15",0,3.6,5005,6305,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FPRX10033050","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.5770000000000001,0.6,"0.90",0.024,"Porsche: Cayenne Turbo, Cayenne Turbo S"]
[2016,"Rolls-Royce","GRRGV06.6N74","GRRGR0170N63","BMW","750i","CY33005",0,4.4,4641,5788,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9RRG10006827","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.028,0.03,"0.05",0,"Rolls-Royce Motor Cars Limited: Dawn, Ghost, Ghost EWB, Wraith"]
[2016,"Subaru","GFJXV02.5PHU","GFJXR01303BC","SUBARU","WRX STI","FBV-UG74",0,2.5,3455,null,3750,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N","FFJX10027871","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28700000000000003,0.29,"0.65",0,"Subaru: WRX"]
[2016,"Toyota","GTYXJ02.5BEL","GTYXR0120A42","TOYOTA","CAMRY","12-AV3A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012669","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","AGED","Aged components installed In the emission data vehicle","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.004,0,"0.20",0,"TOYOTA: CAMRY"]
[2016,"Toyota","GTYXT02.7MER","GTYXR0165P22","TOYOTA","SIENNA","11-AL1A",0,2.672,4275,5895,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","BTYX10007676","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.21300000000000002,0.25,"0.85",0.035,"TOYOTA: TACOMA 4WD"]
[2016,"Toyota","GTYXT04.6BEX","GTYXR0190P32","TOYOTA","TOYOTA TUNDRA 2WD","05-GSK1",2,3.9560000000000004,4270,5700,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","7TYX01071209","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.322,0.36,"1.15",0.035,"LEXUS: GX 460"]
[2016,"Toyota","GTYXT05.7BEW","GTYXR0300P32","TOYOTA","TUNDRA 4WD FFV","15-SK6A",0,5.663,5710,7100,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FTYX10032177","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.011000000000000001,0.01,"0.05",0,"TOYOTA: TUNDRA 2WD, TUNDRA 4WD"]
[2016,"Toyota","GTYXV01.8PC4","GTYXR0130J72","TOYOTA","PRIUS","16-ZV1H",0,1.798,3080,null,3375,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","GTYX10037899","MFR","37","California Fuel Running Loss","46","CARB LEV3 E10 Regular Gasoline","B","AGED","Aged components installed In the emission data vehicle","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL-EQUIV",0,0,"0.05",0,"TOYOTA: PRIUS, PRIUS Eco"]
[2016,"Toyota","GTYXV02.5BED","GTYXR0120A42","TOYOTA","CAMRY","12-AV3A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012669","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","AGED","Aged components installed In the emission data vehicle","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.004,0,"0.20",0,"TOYOTA: CAMRY"]
[2016,"Toyota","GTYXV03.5PC4","GTYXR0155P12","LEXUS","GS 450h","13-GW1H",0,3.456,4190,null,4500,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","DTYX10017497","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24300000000000002,0.28,"0.50",0.035,"LEXUS: GS 450h"]
[2016,"Volkswagen Group of","GVGAJ03.0AUD","GVGAR0140AAD","AUDI","Q5","D3UF-Q5A",0,2.995,4190,5612,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N","DADX10022567","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.025,0.026000000000000002,"0.200",1E-3,"Audi: Q5"]
[2016,"Volkswagen Group of","GVGAV02.0AAC","GVGAR0140NAF","AUDI","A6","D3UF-CAQ",2,2.995,4211,null,4500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"Y","N",null,null,"N","DADX10021118","MFR","37","California Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.007,0.008,"0.050",1E-3,"Audi: A6, A6 quattro"]
[2016,"Volkswagen Group of","GVGAV03.0AUE","GVGAR0155NAH","AUDI","A8","D3UF-DAQ",0,2.995,4553,null,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","DADX10019949","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.031,0.031,"0.200",0,"Audi: A8, A8L"]
[2016,"Volkswagen Group of","GVGAV04.0NUA","GVGAR0140NAE","AUDI","A6","C3UB-CAF",0,1.984,3726,null,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","CADX10012513","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.04,0,"0.2",1E-3,"Audi: RS7, S6, S7"]
[2016,"Volkswagen Group of","GVGAV06.0VLN","GVGAR0130EAN","BENTLEY","PHAETON","611 60011/06",0,5.998,5270,null,5500,"F","2-Wheel Drive, Front","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","8BEX01069616","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.42,0.44,"0.650",0.02,"Bentley: Continental GT, Continental GT Convertible, Flying Spur"]
[2016,"Volvo","GVVXV02.0U3T","GVVXR0130EV3","Volvo","XC60 T6 FWD","201501",0,1.969,3976,5140,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FVVX10028377","MFR","27","California fuel 2-day evap","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","4Z","California LEV-III Zero Evap (Option 2)","150","HC-TOTAL",0.2165,0.265,"0.300",0.0489,"Volvo Cars of North America, LLC: S60 FWD, S60 Inscription FWD, S80 FWD, V60 FWD, XC60 FWD, XC70 FWD"]
[2015,"BMW","FBMXT03.0F15","FBMXR0170N63","BMW","750i","CY33005",0,4.4,4641,5788,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000837","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.01,0.02,"0.20",0.01,"BMW: X5 sDrive35i, X5 xDrive35i, X6 sDrive35i, X6 xDrive35i"]
[2015,"BMW","FBMXV03.0AH5","FBMXR0130AHY","BMW","ActiveHybrid 5","C751520",0,3,4366,5325,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y","CBMX10017566","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.18,0.3,"0.50",0.12,"BMW: ActiveHybrid 5"]
[2015,"BMW","FBMXV04.4N63","FBMXR0130N54","BMW","335i xDrive","KS33736",0,3,3825,4883,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000612","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.012,0.01,"0.05",0,"BMW: 550i, 550i Gran Turismo, 550i xDrive, 550i xDrive Gran Turismo, 650i Convertible, 650i Coupe, 650i Gran Coupe, 650i xDrive Convertible, 650i xDrive Coupe, 650i xDrive Gran Coupe, Alpina B6 Gran Coupe xDrive"]
[2015,"FCA US LLC","FCRXD03.65V0","FCRXR0190TC1","RAM","Promaster 3500","L4VF11444",0,3.6,5066,9350,7000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","ECRX10025967","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.063,0.06,"0.20",0,"RAM: Promaster 1500, Promaster 2500, Promaster 2500 Cab Chassis, Promaster 3500, Promaster 3500 Cab Chassis"]
[2015,"FCA US LLC","FCRXJ01.45P0","FCRXR0116PK1","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017734","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Jeep: Renegade 4x2, Renegade 4x4"]
[2015,"FCA US LLC","FCRXJ02.45P0","FCRXR0116PK1","Dodge","PF","K2PFD4647",0,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","CCRX10017735","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.41200000000000003,0.41000000000000003,"0.65",0,"Jeep: Cherokee 4X4, Cherokee FWD, Renegade 4x4, Renegade Trailhawk 4x4"]
[2015,"FCA US LLC","FCRXJ03.65P0","FCRXR0150RK0","Dodge","CARAVAN 2WD","K8RTY0076",1,3.3000000000000003,4358,6050,4750,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","8CRX01074988","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.313,0.31,"1.15",0,"Chrysler: Town & Country  Dodge: Grand Caravan  RAM: C/V Tradesman"]
[2015,"FCA US LLC","FCRXJ03.65PA","FCRXR0153PKA","Chrysler","SEBRING","K7JSC0306",7,2.7,3457,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01085497","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.39,0.39,"0.85",0,"Dodge: Journey"]
[2015,"FCA US LLC","FCRXT02.45P1","FCRXR0112PK0","Dodge","CALIBER AWD","K6PMD5278",0,2,3065,4435,3375,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"Y","N","SF","Single Fuel","N","8CRX01066883","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.462,0.46,"0.65",0,"Jeep: Compass FWD, Patriot FWD"]
[2015,"FCA US LLC","FCRXT03.65PD","FCRXR0225RKA","Dodge","Ram 1500 Pickup 4wd","K9DS16774",0,4.7,5489,6800,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01086623","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.8560000000000001,0.86,"0.90",0,"RAM: 1500 4X2, 1500 4X4"]
[2015,"FCA US LLC","FCRXT05.75P0","FCRXR0190RK0","Dodge","Ram 1500 Pickup 4wd","K9DS16740",0,4.7,5489,6800,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01086066","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.51,0.51,"0.90",0,"RAM: 1500 4X2, 1500 4X4"]
[2015,"Ferrari","FFEXV04.3GDI","FFEXR0175149","Ferrari","458 Italia Spyder","ZFF67NHB000171765",0,4.5,3495,4046,3875,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N","AFEX10008691","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.218,0.22,"0.65",0,"Ferrari North America, Inc.: 458 Italia, 458 Speciale, 458 Speciale Spider, 458 Spider"]
[2015,"FOMOCO","FFMXD03.57BT","FFMXR0190NBD","Ford","T350 FFV Van","ETH1-3.7-J-465",0,3.7,6925,9500,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10028137","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.35400000000000004,0.35000000000000003,"1.00",0,"Ford: Transit T350 Van, Transit T350 Wagon"]
[2015,"FOMOCO","FFMXT01.62E9","FFMXR0125NBV","Ford","Escape AWD","DM21-1.6-F-223",0,1.6,3714,4770,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DFMX10018869","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"000.05",2E-3,"Ford: ESCAPE AWD, ESCAPE FWD"]
[2015,"FOMOCO","FFMXT02.73JJ","FFMXR0160ABC","Ford","F-150 Super Cab Max","FFC1-2.7-F-545",0,2.7,4932,7000,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FFMX10031879","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.334,0.33,"0.90",0,"Ford: F150 PICKUP 2WD, F150 PICKUP 4WD, F150 SFE PICKUP 2WD"]
[2015,"FOMOCO","FFMXT03.53DC","FFMXR0160ABC","Ford","F-150 4X4","FFC1-5.0-554",0,5,5260,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10033208","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.397,0.4,"0.90",0,"Ford: F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2015,"FOMOCO","FFMXT05.03DK","FFMXR0160ABC","Ford","F-150 4X4","FFC1-5.0-554",0,5,5260,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10033207","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"000.05",0,"Ford: F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2015,"FOMOCO","FFMXT05.03DK","FFMXR0235NBC","Ford","F-150 4X4","FFC1-5.0-J-550",0,5,5260,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","FFMX10033167","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.618,0.62,"0.90",0,"Ford: F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2015,"FOMOCO","FFMXV01.6VDD","FFMXR0105GBA","Ford","Fiesta ST","ECT2-1.6-407",1,1.6,2720,4279,3000,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N","EFMX10024053","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.3,0.32,"0.50",0.022000000000000002,"Ford: Fiesta ST FWD"]
[2015,"FOMOCO","FFMXV02.3VJW","FFMXR0125NBV","Ford","Mustang","FZG1-3.7-C-559",0,3.7,3711,4560,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FFMX10030994","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"000.05",2E-3,"Ford: MUSTANG, MUSTANG CONVERTIBLE, MUSTANG SFE"]
[2015,"FOMOCO","FFMXV03.7VE8","FFMXR0145GBV","FORD","FREESTYLE AWD","8P51-3.5-F-509",4,3.5,4431,5460,4750,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","AFMX01073447","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.34900000000000003,0.35000000000000003,"000.50",0,"Ford: FLEX AWD, Flex FWD, Police Interceptor Sedan AWD, Police Interceptor Sedan FWD, TAURUS AWD, TAURUS FWD  Lincoln: MKS AWD, MKS FWD, MKT FWD, MKT LIVERY AWD"]
[2015,"GM","FGMXJ02.4199","FGMXR0138813","CHEVROLET","TLJ26","30TALP5135",0,3,4243,5300,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AGMX10002235","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.036000000000000004,0.04,"0.20",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2015,"GM","FGMXJ03.6165","FGMXR0120818","CHEVROLET","1ND69","2215NP4000",1,2,3339,4240,3625,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061625","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.58,0.58,"0.65",0,"Cadillac: ATS, ATS AWD"]
[2015,"GM","FGMXJ03.6165","FGMXR0170956","CADILLAC","SRX 2WD","366CNN4028",0,3.6,4544,5555,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","CGMX10012681","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0,0,"0.05",0,"Cadillac: SRX, SRX AWD"]
[2015,"GM","FGMXT03.6151","FGMXR0138813","GMC","CANYON 4WD","36SPFN1011",0,3.6,4540,6000,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FGMX10031493","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.232,0.23,"0.65",0,"Chevrolet: COLORADO CAB CHASSIS 2WD  GMC: CANYON CAB CHASSIS 2WD"]
[2015,"GM","FGMXT05.3382","FGMXR0176820","CHEVROLET","CC10706","53XECU7422",1,5.3,5217,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01066640","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.547,0.55,"0.90",0,"Chevrolet: C15 SILVERADO 2WD, C1500 TAHOE 2WD, K15 SILVERADO 4WD, K1500 TAHOE 4WD  GMC: C15 SIERRA 2WD, C1500 YUKON 2WD, K15 SIERRA 4WD, K1500 YUKON 4WD"]
[2015,"GM","FGMXV01.4001","FGMXR0060800","CHEVROLET","VOLT","141CRN4523",0,1.4000000000000001,3694,null,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","BGMX10010913","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",2E-3,0,"0.05",0,"Chevrolet: VOLT"]
[2015,"GM","FGMXV01.4088","FGMXR0060600","CHEVROLET","VOLT","141CRN4523",1,1.4000000000000001,3715,null,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","CGMX91001175","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.13,0.17,"0.65",0.04,"Cadillac: ELR  Chevrolet: VOLT"]
[2015,"GM","FGMXV02.0021","FGMXR0120818","CHEVROLET","1ND69","2215NP4000",1,2,3339,4240,3625,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061626","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.343,0.34,"0.50",0,"Buick: VERANO  Cadillac: ATS, ATS AWD"]
[2015,"GM","FGMXV03.6048","FGMXR0123702","CHEVROLET","2WS69","3825WN4008",31,3.5,3629,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01061189","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.17800000000000002,0.22,"0.35",0.04,"Buick: LACROSSE  Cadillac: XTS  Chevrolet: IMPALA"]
[2015,"GM","FGMXV06.2087","FGMXR0133880","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017013","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.20500000000000002,0.2,"0.50",0,"Cadillac: CTS"]
[2015,"GM","FGMXV06.2089","FGMXR0133880","CHEVROLET","1WB19","3516WN4002",1,3.5,3579,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX10001398","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"0.05",0,"Chevrolet: CAMARO"]
[2015,"Honda","FHNXV01.51H2","FHNXR0086VFA","HONDA","FIT EX","EFR72C",0,1.5,2627,null,2875,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N","FHNX91002061","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.448,0.52,"0.65",0.07,"Honda: FIT"]
[2015,"Honda","FHNXV01.5PFB","FHNXR0106VFA","ACURA","ILX","ED9A2A",0,2,3018,null,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,5,"Y","N",null,null,"N","DHNX10019080","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.032,0.03,"0.20",0,"Honda: CIVIC HYBRID"]
[2015,"Honda","FHNXV02.4DA3","FHNXR0151VFA","HONDA","ACCORD EX/EX-L SEDAN","E8422A",0,2.4,3485,null,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,5,"Y","N","SF","Single Fuel","N","8HNX01076410","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",2E-3,0,"0.20",0,"Honda: CROSSTOUR 2WD"]
[2015,"Honda","FHNXV03.5WA4","FHNXR0121VFA","ACURA","TLX","EFJ24A",0,3.5,3789,null,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","FHNX10031138","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Acura: TLX"]
[2015,"Hyundai","FHYXT02.42UP","FHYXR01372U3","Hyundai","Tucson","LM4F4GG31B1",0,2.4,3477,4608,3750,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","EHYX10025697","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.007,0.01,"0.20",0,"HYUNDAI MOTOR COMPANY: Tucson AWD"]
[2015,"Hyundai","FHYXV03.81PE","FHYXR0140ARE","HYUNDAI","Genesis","DH5T0GU11A2",0,5,4724,5710,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FHYX10028453","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.2904,0.29,"0.500",0,"HYUNDAI MOTOR COMPANY: Genesis AWD, Genesis RWD"]
[2015,"Jaguar Land Rover L","FJLXT02.0FTP","FJLXR0140P1Z","Land Rover","Range Rover Evoque","3EVPP037",0,2,3995,5181,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,9,"Y","N",null,null,"N","EJLX10028183","MFR","24","Federal fuel refueling test (ORVR)","47","CARB LEV3 E10 Premium Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.009000000000000001,0.01,"0.20",0,"Land Rover: Discovery Sport, Range Rover Evoque"]
[2015,"Kia","FKMXT02.04ME","FKMXR0132DME","KIA","Sportage","SL1F0HU15A1",0,2,3605,4696,3875,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","BKMX91000825","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.41700000000000004,0.42,"0.85",0,"KIA MOTORS CORPORATION: Sportage AWD, Sportage FWD, Sportage SX AWD, Sportage SX FWD"]
[2015,"Kia","FKMXV01.84EE","FKMXR01284EE","KIA","Forte ECO","YD3N8GF23A1",0,1.8,2820,3880,3125,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10023376","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.323,0.32,"0.50",0,"KIA MOTORS CORPORATION: Forte"]
[2015,"Kia","FKMXV01.85EP","FKMXR01345E3","KIA","Forte ECO","YD3N8GU21A1",0,1.8,2820,3880,3125,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10023367","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.041,0.04,"0.20",0,"KIA MOTORS CORPORATION: Forte"]
[2015,"Kia","FKMXV03.34KE","FKMXR01394KE","Kia","Cadenza","VG4L3AU21A2",0,3.3000000000000003,3792,4696,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10023303","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.193,0.19,"0.50",0,"KIA MOTORS CORPORATION: Cadenza"]
[2015,"Lotus","FLTXV03.5JHB","FLTXR0130JHB","LOTUS","EVORA","EDV-10-EVM6S",1,3.5,3047,3375,3375,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","ALTX10010206","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.3,"0.5",0.013000000000000001,"Lotus Cars Ltd: Evora"]
[2015,"MAZDA","FTKXV02.5NC1","FTKXR0115GCX","MAZDA","MAZDA6","4ECPY31-009",1,2.5,3183,4226,3500,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N","ETKX10023002","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.05",0,"MAZDA: MAZDA3 4-Door, MAZDA3 5-Door"]
[2015,"Mercedes-Benz","FMBXJ02.0U2A","FMBXR0110LNF","Mercedes-Benz","B 250","W246E20DETC-Z3021",0,1.991,3293,4409,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,7,"Y","N",null,null,"N","DMBX10022551","MFR","34","Federal fuel 3-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.327,0.33,"0.50",0,"Mercedes-Benz: B 250, B 250 4MATIC, CLA 250, CLA 250 4MATIC, GLA 250, GLA 250 4MATIC"]
[2015,"Mercedes-Benz","FMBXJ03.5U2A","FMBXR0170LNF","Mercedes-Benz","ML 350 4MATIC","W166E35DEH-Z2036",1,3.498,4813,6283,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","CMBX10018716","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.008,0.01,"0.05",0,"Mercedes-Benz: ML 350 4MATIC"]
[2015,"Mercedes-Benz","FMBXV03.5HY1","FMBXR0168LNP","Mercedes-Benz","E 400 HYBRID","W212E35DEH Hyb-Z3017",0,3.498,4235,5203,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"Y","DMBX10022582","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.27,0.31,"0.35",0.038,"Mercedes-Benz: E 400 Hybrid"]
[2015,"Mercedes-Benz","FMBXV03.5U2C","FMBXR0155LNS","Mercedes-Benz","SL 600","R230E55TC-Z7019",0,5.513,4519,5095,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","AMBX10002172","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Mercedes-Benz: SLK 350"]
[2015,"Mitsubishi Motors Co","FMTXT02.4GEZ","FMTXR0135A1D","MITSUBISHI","LANCER","EB08-CA32",0,1.998,2922,4079,3250,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N","AMTX10003928","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.009000000000000001,0.012,"0.050",0.003,"Mitsubishi Motors Corporation: OUTLANDER SPORT 2WD, OUTLANDER SPORT 4WD, RVR 2WD, RVR 4WD"]
[2015,"Mitsubishi Motors Co","FMTXT03.0GEX","FMTXR0135A1D","MITSUBISHI","LANCER","EB08-CA32",0,1.998,2922,4079,3250,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N","AMTX10003926","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.12100000000000001,0.12100000000000001,"0.650",0,"Mitsubishi Motors Corporation: OUTLANDER 4WD"]
[2015,"Nissan","FNSXD05.6Y9A","FNSXF0174PBA","NISSAN","NISSAN NV3500 M S/R","TYB016",0,5.6000000000000005,6187,9900,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","CNSX10011383","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","HD-2D","Federal Heavy-Duty 2-Day Evap (1.75 grams)","120","HC-TOTAL",0.627,0.63,"1.75",0,"NISSAN: NV2500 Cargo Van, NV3500 Cargo Van, NV3500 Passenger Van"]
[2015,"Nissan","FNSXT04.0G6A","FNSXR0132PBA","NISSAN","NISSAN FRONTIER 4WD C/C PRO-4X","SRE410",1,4,4567,5599,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N",null,null,"N","DNSX10022766","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.061000000000000006,0.06,"0.20",0,"NISSAN: FRONTIER 2WD, FRONTIER 4WD, XTERRA 2WD, XTERRA 4WD"]
[2015,"Nissan","FNSXT05.6G9D","FNSXR0174PBC","INFINITI","INFINITI QX56 4WD","TWB022",1,5.6000000000000005,5878,7500,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,7,"Y","N","SF","Single Fuel","N","BNSX10007705","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.023,0.02,"0.20",0,"INFINITI: QX80 4WD"]
[2015,"Nissan","FNSXV02.585A","FNSXR0120PBA","NISSAN","NISSAN ALTIMA 3.5SL","FPB064",0,3.5,3375,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","DNSX91001351","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRA","Mfr. Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.163,0.16,"0.65",0,"NISSAN: ALTIMA"]
[2015,"Nissan","FNSXV05.6G9A","FNSXR0120MBB","INFINITI","INFINITI M56X Base","DNB138",0,5.6000000000000005,4250,null,4500,"4","4-Wheel Drive","SA","Semi-Automatic",null,7,"Y","N","SF","Single Fuel","N","BNSX10006610","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",1E-3,0,"0.05",0,"INFINITI: Q70, Q70 AWD"]
[2015,"Porsche","FPRXT03.6MCS","FPRXR0230RED","Porsche","Cayenne S","EC-92AIIS-15",0,3.6,5005,6305,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","FPRX10033050","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.5770000000000001,0.62,"0.65",0.047,"Porsche: Cayenne S"]
[2015,"Porsche","FPRXV04.8PS8","FPRXR0200RPD","Porsche","Panamera 4S Executive","EC-970IIS-14",0,3,4488,5478,4750,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","EPRX10027360","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Porsche: Panamera GTS"]
[2015,"Roush","FRIIV05.0VIM","FRIIR0125NDA","Ford","Mustang","FZG1-3.7-C-559",0,3.7,3711,4560,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FFMX10031806","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.01,0.01,"0.20",0,"Roush Industries, Inc.: Roush Stage 3 Mustang"]
[2015,"Toyota","FTYXT02.0KEM","FTYXR0132A22","LEXUS","NX 200t AWD F SPORT","15-AZ1A",0,1.998,4050,5200,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","FTYX10032343","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.2,0.2,"0.65",0,"LEXUS: NX 200t, NX 200t AWD, NX 200t AWD F SPORT"]
[2015,"Toyota","FTYXT02.7BEP","FTYXR0165A22","LEXUS","SC 430","06-UZ1A",0,4.293,3890,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","6TYX01063443","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.021,0.04,"0.20",0.017,"TOYOTA: VENZA, VENZA 4WD"]
[2015,"Toyota","FTYXT03.5CC4","FTYXR0160E52","LEXUS","RX 400h 4WD","06-MU1C",0,3.311,4520,5490,4750,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","6TYX10000172","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.007,0.01,"0.05",0,"LEXUS: RX 450h, RX 450h AWD"]
[2015,"Toyota","FTYXT05.7BEW","FTYXR0300P32","TOYOTA","TUNDRA 4WD FFV","15-SK6A",0,5.663,5710,7100,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","FTYX10032177","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","AGED","Aged components installed In the emission data vehicle","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.011000000000000001,0.01,"0.05",0,"TOYOTA: TUNDRA 2WD, TUNDRA 4WD"]
[2015,"Toyota","FTYXV01.5BEB","FTYXR0085P12","SCION","iQ","11-NJ2C",0,1.329,2135,null,2375,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N","SF","Single Fuel","N","BTYX10009641","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",1E-3,0,"0.05",0,"TOYOTA: YARIS"]
[2015,"Toyota","FTYXV02.5BEB","FTYXR0115P12","SCION","tC","11-AT1M",0,2.494,3110,null,3375,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N","SF","Single Fuel","N","BTYX10009496","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",1E-3,0.01,"0.20",0.013000000000000001,"SCION: tC"]
[2015,"Toyota","FTYXV03.5BEC","FTYXR0115A12","TOYOTA","CAMRY","12-AV1A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012590","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.023,0.04,"0.20",0.017,"LEXUS: ES 350  TOYOTA: AVALON, CAMRY"]
[2015,"Toyota","FTYXV05.0CC4","FTYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008779","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.17,0.17,"0.65",0,"LEXUS: LS 600h L"]
[2015,"Volkswagen Group of","FVGAT03.0ALT","FVGAR0170NAM","AUDI","Q7","7358-TAQ",1,4.163,5501,null,6000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01067969","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.47000000000000003,0.5,"0.9",0.013000000000000001,"Audi: Q7"]
[2015,"Volkswagen Group of","FVGAV02.0APA","FVGAR0110ABB","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.05",0,"Audi: A3, A3 Cabriolet, A3 Cabriolet quattro, A3 quattro  Volkswagen: GTI, Golf, Golf SportWagen"]
[2015,"Volkswagen Group of","FVGAV02.0VBD","FVGAR0110VAD","VOLKSWAGEN","JETTA","351 750 101/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061093","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.01,0,"0.2",0,"Volkswagen: Beetle, Beetle Convertible, Jetta"]
[2015,"Volkswagen Group of","FVGAV04.0NUA","FVGAR0155NAH","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX91000564","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.432,0.45,"0.65",0.018000000000000002,"Audi: A8, A8L"]
[2015,"Volkswagen Group of","FVGAV04.2NLC","FVGAR0130NAJ","AUDI","R8","8375-RAQ",1,4.163,3671,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01076741","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.405,0.42200000000000004,"0.500",0.017,"Audi: R8, R8 Spyder"]
[2015,"Volvo","FVVXJ03.0U2T","FVVXR0130EV2","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003728","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.382,0.382,"0.650",0,"Volvo Cars of North America, LLC: S60 AWD, S60 PoleStar AWD, V60 AWD, V60 PoleStar AWD"]
[2014,"aston martin","EASXV04.7VH2","EASXR0160P1Y","Aston Martin","V8 Vantage","FEU06",0,4.3,3461,4035,3750,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","6ASX10000030","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Aston Martin Lagonda Ltd: V8 Vantage, V8 Vantage S"]
[2014,"Audi","EADXV02.03PA","EADXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: GTI"]
[2014,"Audi","EADXV04.03UJ","EADXR0155D4A","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX10008832","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.43,0.4,"0.5",0.018000000000000002,"Audi: A8, A8L"]
[2014,"Audi","EADXV05.2LR8","EADXR0130R8A","AUDI","R8","8375-RAQ",1,4.163,3671,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01076741","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.405,0.42200000000000004,"0.500",0.017,"Audi: R8, R8 Spyder  Lamborghini: Gallardo Coupe, Gallardo Spyder"]
[2014,"BMW","EBMXT04.4F15","EBMXR0170N63","BMW","750i","CY33005",0,4.4,4641,5788,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000837","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.01,0.02,"0.20",0.01,"BMW: X5 xDrive50i, X6 xDrive50i"]
[2014,"BMW","EBMXV04.4N63","EBMXR0130N54","BMW","335i xDrive","KS33736",0,3,3825,4883,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9BMX10000612","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0.012,0.01,"0.05",0,"BMW: 550i, 550i Gran Turismo, 550i xDrive, 550i xDrive Gran Turismo, 650i Convertible, 650i Coupe, 650i Gran Coupe, 650i xDrive Convertible, 650i xDrive Coupe, 650i xDrive Gran Coupe"]
[2014,"Falcon Lab LLC","EFLCT04.0KEK","EFLCR0049PBN","CHRYSLER","JEEP CHEROKE","1J4FN68S8VL589304",0,4,3153,4949,3750,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","BUSD10029339","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","T1","Federal Tier 1 Evap","100","HC-TOTAL",0.46,0.5,"2.0",null,"Falcon Labs: 1997 Jeep Cherokee"]
[2014,"FCA US LLC","ECRXD06.45W1","ECRXF0205TC0","Dodge","RAM 3500 CAB CHAS 2WD","K7DC88916",0,5.7,10000,12500,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","9CRX01070371","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.754,0.79,"1.75",0.04,"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2014,"FCA US LLC","ECRXJ03.65PA","ECRXR0130PKA","Chrysler","SEBRING","K7JSC0306",7,2.7,3457,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX10000295","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"0.05",0,"Chrysler: 200, 200 Convertible  Dodge: Avenger"]
[2014,"FCA US LLC","ECRXT03.65P0","ECRXR0150RK0","Chrysler","TOWN & COUNTRY FWD","K8RTY0076",0,3.3000000000000003,4457,6050,4750,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01074987","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.065,0.06,"0.20",0,"Chrysler: Town & Country  Dodge: Grand Caravan  RAM: C/V"]
[2014,"FCA US LLC","ECRXT03.65P1","ECRXR0225RK0","Dodge","Ram 1500 Pickup 4wd","K9DS16774",0,4.7,5489,6800,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01086214","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.49200000000000005,0.5,"1.15",0.01,"RAM: 1500 4X2, 1500 4X4"]
[2014,"FCA US LLC","ECRXT03.65PC","ECRXR0190RKA","Dodge","Ram 1500 Pickup 4wd","K9DS16740",0,4.7,5489,6800,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","9CRX01086066","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.51,0.51,"0.90",0,"RAM: 1500 4X2, 1500 4X4"]
[2014,"FCA US LLC","ECRXV02.05PA","ECRXR0116PKA","Dodge","Dart","L2PFD3317",0,2,3260,4285,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","DCRX10022887","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.17800000000000002,0.2,"0.20",0.02,"Dodge: Dart"]
[2014,"FCA US LLC","ECRXV03.65PA","ECRXR0145PKA","Chrysler","300 AWD","L8LXC9919",6,5.7,4386,5500,4750,"A","All Wheel Drive","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","9CRX10000419","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Chrysler: 300, 300 AWD  Dodge: Charger, Charger AWD"]
[2014,"Ferrari","EFEXV06.3HYB","EFEXR017512C","Ferrari","FF","ZFFJY54B000168921",0,6.3,4189,5115,4750,"P","Part-time 4-Wheel Drive","AM","Automated Manual",null,7,"N","N",null,null,"N","CFEX10016604","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.338,0.34,"0.50",0,"Ferrari North America, Inc.: LaFerrari"]
[2014,"FOMOCO","EFMXT02.52ET","EFMXR0125NBV","Ford","Escape AWD","DM21-1.6-F-223",0,1.6,3714,4770,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DFMX10018869","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"000.05",2E-3,"Ford: ESCAPE FWD"]
[2014,"FOMOCO","EFMXT03.73E8","EFMXR0145GBV","FORD","FREESTYLE AWD","8P51-3.5-F-509",4,3.5,4431,5460,4750,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","AFMX01073444","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.34900000000000003,0.35000000000000003,"000.65",0,"Ford: EXPLORER AWD, EXPLORER FWD, Police Interceptor Utility AWD, Police Interceptor Utility FWD"]
[2014,"FOMOCO","EFMXT06.27HL","EFMXR0250NBS","Ford","F350 4x4","BFA1-6.2-J-007",0,6.2,9090,11200,9500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BFMX10006388","MFR","24","Federal fuel refueling test (ORVR)","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.013000000000000001,0.04,"0.20",0.026000000000000002,"Ford: F250 PICKUP 2WD FFV, F250 PICKUP 4WD FFV, F350 Pickup 2WD FFV, F350 Pickup 4WD FFV"]
[2014,"FOMOCO","EFMXV01.6VDD","EFMXR0105GBA","Ford","FIESTA","ECT3-1.6-J-404",0,1.6,2631,3620,3000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EFMX10023106","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.005,0,"0.20",0,"Ford: Fiesta ST FWD"]
[2014,"FOMOCO","EFMXV02.0VZS","EFMXR0105GDA","Ford","MKZ (HEV)","DC91-2.0-J-268",0,2,3912,4250,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y","DFMX10020812","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"000.05",0,"Ford: FUSION HYBRID FWD  Lincoln: MKZ HYBRID FWD"]
[2014,"FOMOCO","EFMXV03.7VE8","EFMXR0145GBV","FORD","FREESTYLE AWD","8P51-3.5-F-509",4,3.5,4431,5460,4750,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","AFMX01073474","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.021,0.02,"000.20",0,"Ford: FLEX AWD, FLEX FWD, Police Interceptor Sedan AWD, Police Interceptor Sedan FWD, TAURUS AWD, TAURUS FWD  Lincoln: MKS AWD, MKS FWD, MKT FWD, MKT LIVERY AWD"]
[2014,"GM","EGMXJ02.4199","EGMXR0133810","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017012","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.28800000000000003,0.29,"0.65",0,"Buick: REGAL  Chevrolet: ORLANDO"]
[2014,"GM","EGMXJ03.6165","EGMXR0138813","GMC","TERRAIN AWD","30TALP5135",1,3,4197,5300,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BGMX10008884","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.35200000000000004,0.35000000000000003,"0.85",0,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2014,"GM","EGMXT02.4151","EGMXR0138813","GMC","TERRAIN AWD","30TALP5135",1,3,4197,5300,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","BGMX10008882","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0,0,"0.05",0,"Chevrolet: CAPTIVA FWD, EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2014,"GM","EGMXT05.3373","EGMXR0176820","CHEVROLET","RN15306","37XEHU7006",2,2.9,3932,5300,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01067513","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.015000000000000001,0.02,"0.20",0,"Chevrolet: C10 TAHOE 2WD, K10 TAHOE 4WD  GMC: C10 YUKON 2WD, K10 YUKON  4WD"]
[2014,"GM","EGMXT05.3381","EGMXR0223840","CHEVROLET","CC10903","53XECP8101",0,5.3,5950,7300,6000,"A","All Wheel Drive","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01075229","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0.762,0.76,"1.15",0,"Chevrolet: C10 AVALANCHE 2WD, C10 SUBURBAN 2WD, K10 AVALANCHE 4WD, K10 SUBURBAN 4WD  GMC: C10 YUKON  XL 2WD, K10 YUKON XL 4WD"]
[2014,"GM","EGMXT05.3382","EGMXR0223840","GMC","CC15903","43XECP6053",6,4.8,5727,9600,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01068129","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.7070000000000001,0.71,"0.90",0,"Chevrolet: C15 SILVERADO 2WD, C1500 SUBURBAN 2WD, K15 SILVERADO 4WD, K1500 SUBURBAN 4WD  GMC: C15 SIERRA 2WD, C1500 YUKON XL 2WD, K15 SIERRA 4WD, K1500 YUKON XL 4WD"]
[2014,"GM","EGMXT06.2374","EGMXR0223840","CHEVROLET","CC10903","53XECP8101",0,5.3,5950,7300,6000,"A","All Wheel Drive","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01075229","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.762,0.76,"1.15",0,"Cadillac: ESCALADE ESV 2WD, ESCALADE ESV 4WD  GMC: C1500 YUKON XL 2WD, K1500 YUKON XL 4WD"]
[2014,"GM","EGMXT06.2375","EGMXR0223840","CHEVROLET","CC10903","53XECP8101",0,5.3,5950,7300,6000,"A","All Wheel Drive","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX10002177","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","OMHCE",0,0,"0.05",0,"Cadillac: ESCALADE ESV 2WD, ESCALADE ESV AWD  GMC: C10 YUKON  XL 2WD, K10 YUKON XL AWD"]
[2014,"GM","EGMXV02.0021","EGMXR0133810","BUICK","4HP69","3846HN4008",13,3.9,3824,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01062010","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.011000000000000001,0.01,"0.20",0,"Buick: REGAL, REGAL AWD  Cadillac: CTS SEDAN, CTS SEDAN AWD  Chevrolet: MALIBU"]
[2014,"GM","EGMXV02.4069","EGMXR0117704","CHEVROLET","1AZ69","2217AN4002",1,2.2,2949,null,3250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX10001329","MFR","32","Federal Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Buick: LACROSSE, REGAL  Chevrolet: IMPALA, MALIBU"]
[2014,"GM","EGMXV03.6167","EGMXR0133810","BUICK","LACROSSE","244BGN4226",2,2.4,3777,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y","CGMX10017012","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28800000000000003,0.29,"0.65",0,"Cadillac: XTS, XTS HEARSE, XTS LIMO"]
[2014,"GM","EGMXV06.2089","EGMXR0133880","CHEVROLET","1WB19","3516WN4002",1,3.5,3579,null,3875,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N","AGMX01062382","MFR","23","2-day evap","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","OMHCE",0.29600000000000004,0.3,"0.65",0,"Chevrolet: CAMARO"]
[2014,"GM","EGMXV07.0088","EGMXR0133880","BUICK","4HP69","3846HN4008",13,3.9,3824,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N","AGMX01062010","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.011000000000000001,0.01,"0.20",0,"Chevrolet: CAMARO, CHEV SS"]
[2014,"Honda","EHNXT03.5JT3","EHNXR01351FA","ACURA","RDX 4WD","ED8A3A",0,3.5,3901,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DHNX10018366","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.012,0.01,"0.20",0,"Acura: RDX 2WD, RDX 4WD"]
[2014,"Honda","EHNXV01.8FB2","EHNXR0106VFA","ACURA","ILX","ED9A2A",0,2,3018,null,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,5,"Y","N",null,null,"N","DHNX10019080","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.032,0.03,"0.20",0,"Honda: CIVIC, CIVIC HF"]
[2014,"Honda","EHNXV02.0ZG2","EHNXR0129VGA","HONDA","ACCORD HYBRID","EEK12C",0,2,3620,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y","EHNX91001852","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.189,0.2,"0.65",0.01,"Honda: ACCORD"]
[2014,"Honda","EHNXV03.52G2","EHNXR0129VFA","ACURA","RLX HYBRID","EE9S2A",0,3.5,4357,null,4750,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","EHNX10027511","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Acura: RLX"]
[2014,"Hyundai","EHYXT02.42UP","EHYXR01372U3","Hyundai","Tucson","LM4F4GG31B1",0,2.4,3477,4608,3750,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","EHYX10025696","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.017,0.017,"0.050",0,"HYUNDAI MOTOR COMPANY: Tucson 4WD"]
[2014,"Hyundai","EHYXV02.01VE","EHYXR0130AVE","Hyundai","Santa Fe Sport","AN3F0HU17A1",0,2,3878,5181,4250,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N","DHYX91001402","EPA","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.5005000000000001,0.5,"0.650",0,"HYUNDAI MOTOR COMPANY: Santa Fe Sport 2WD, Santa Fe Sport 4WD"]
[2014,"Hyundai","EHYXV05.01SE","EHYXR0140ARE","HYUNDAI","GENESIS R SPEC","BH2T0GU33A2",0,5,4147,5115,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","CHYX10012334","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.020800000000000003,0.021,"0.050",0,"HYUNDAI MOTOR COMPANY: EQUUS"]
[2014,"Jaguar Land Rover L","EJLXT03.0002","EJLXR0175001","Land Rover","Range Rover","LKDMP2001",0,5,5404,6724,5500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N","EJLX10026606","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.02,0,"0.2",0,"Land Rover: Range Rover FFV, Range Rover L FFV, Range Rover Sport FFV"]
[2014,"Kia","EKMXV01.64DE","EKMXR01284DE","KIA","Forte5","YD3R6AU09A1",0,1.6,3025,4056,3375,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10025129","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.021,0.021,"0.050",0,"KIA MOTORS CORPORATION: Forte 5, Forte Koup"]
[2014,"Kia","EKMXV01.8DEE","EKMXR01284EE","KIA","Forte ECO","YD3N8GF23A1",0,1.8,2820,3880,3125,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","EKMX10023376","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.323,0.323,"0.500",0,"KIA MOTORS CORPORATION: Forte, Forte ECO"]
[2014,"Kia","EKMXV02.44HE","EKMXR0140DHE","KIA","OPTIMA","TF1F4AU31A1",0,2.4,3230,4299,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","BKMX10009089","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.41600000000000004,0.41600000000000004,"0.650",0,"KIA MOTORS CORPORATION: OPTIMA"]
[2014,"Maserati","EMAXV03.8DFI","EMAXR0136DFI","MASERATI","QUATTROPORTE GTS","066158",0,3.8000000000000003,4495,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N","EMAX10025844","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.036000000000000004,0.06,"0.20",0.02,"MASERATI: QUATTROPORTE GTS"]
[2014,"MAZDA","ETKXT03.75BA","ETKXR0145GAL","FORD","MAZDA CX-9","7J51-3.5-F-743",0,3.5,4564,4750,4750,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9FMX10002850","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"MAZDA: CX-9 2WD, CX-9 4WD"]
[2014,"McLaren Automotive ","EMLNV03.8MA2","EMLNR0164MB3","McLaren","P1","SBM12ABA7EW990019",0,3.7990000000000004,3296,null,3625,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"N","N",null,null,"Y","EMLN10029001","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.009000000000000001,0.01,"0.05",0,"McLaren Automotive Limted: P1"]
[2014,"Mercedes-Benz","EMBXT03.5U2A","EMBXR0170LNC","Mercedes-Benz","G 550","G463E55-Z9017-1",0,5.461,5699,6613,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N","SF","Single Fuel","N","9MBX10000078","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","OT","Other","50","NMOG",0.021500000000000002,0.032,"0.040",0.0109,"Mercedes-Benz: ML 350, ML 350 4MATIC"]
[2014,"Mercedes-Benz","EMBXT05.5U2B","EMBXR0170LNC","Mercedes-Benz","G 550","G463E55-Z9017-1",0,5.461,5699,6613,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N","SF","Single Fuel","N","9MBX10000041","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","OT","Other","50","NOX",0.016,0.02,"0.05",0.007,"Mercedes-Benz: G 550"]
[2014,"Mercedes-Benz","EMBXV03.5U2B","EMBXR0160LNF","Mercedes-Benz","E 350 4 MATIC","W212E35DEH-Z2004-6",0,3.498,4255,5225,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N","DMBX10024122","MFR","32","Federal Fuel Running Loss","37","E10 (10% Ethanol 90% EPA Unleaded Gasoline)","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Mercedes-Benz: C 300 4MATIC, E 350 4MATIC (coupe)"]
[2014,"Mercedes-Benz","EMBXV05.5U2A","EMBXR0170LNS","Mercedes-Benz","S 600","V221E55TC-Z7014",0,5.513,5037,5390,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","AMBX10003171","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Mercedes-Benz: CL 550 4MATIC, CL 63 AMG, S 63 AMG 4MATIC"]
[2014,"Mitsubishi Motors Co","EMTXV02.0GRB","EMTXR0135A1C","MITSUBISHI","LANCER EVOLUTION","EB08-CA62",1,1.998,3517,4542,3875,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N","AMTX10003939","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.277,0.277,"0.650",0,"Mitsubishi Motors Corporation: LANCER, LANCER EVOLUTION, LANCER SPORTBACK"]
[2014,"Nissan","ENSXD04.0Y6B","ENSXF0174PBA","NISSAN","NISSAN NV3500 M S/R","TYB016",0,5.6000000000000005,6187,9900,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","CNSX10011387","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","HD-3D","Federal Heavy-Duty 3-Day Evap (1.4 grams)","120","HC",0.003,0,"0.05",0,"NISSAN: NV1500 Cargo Van, NV2500 Cargo Van, NV3500 Passenger Van"]
[2014,"Nissan","ENSXT03.5G7A","ENSXR0120PBB","INFINITI","INFINITI JX35 AWD","GJB181",0,3.5,4497,5937,4750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N","DNSX10017320","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.314,0.31,"0.85",0,"INFINITI: QX60 AWD, QX60 FWD  NISSAN: PATHFINDER 2WD, PATHFINDER 4WD, QUEST"]
[2014,"Nissan","ENSXT05.6G9C","ENSXR0174PBC","INFINITI","INFINITI QX56 4WD","TWB022",0,5.6000000000000005,5878,7500,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,7,"Y","N","SF","Single Fuel","N","BNSX10007821","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.331,0.33,"0.90",0,"INFINITI: QX80 2WD, QX80 4WD"]
[2014,"Nissan","ENSXV01.8G1B","ENSXR0090PBA","NISSAN","NISSAN SENTRA 2.0SL","AWE259",0,2,3013,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N","SF","Single Fuel","N","9NSX01087123","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.332,0.33,"0.50",0,"NISSAN: CUBE"]
[2014,"Nissan","ENSXV03.8GBA","ENSXR0132MBB","NISSAN","GT-R","MNB211",1,3.8000000000000003,3887,null,4250,"4","4-Wheel Drive","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9NSX01081503","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.011000000000000001,0.01,"0.20",0,"NISSAN: GT-R"]
[2014,"Porsche","EPRXT04.8CSD","EPRXR0230RED","Porsche","Cayenne S","EC48SA-7",0,4.8,5269,6790,6000,"A","All Wheel Drive","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","APRX10001879","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.017,0.02,"0.20",0.005,"Porsche: Cayenne GTS, Cayenne S"]
[2014,"Porsche","EPRXV03.0PTD","EPRXR0200RPD","Porsche","Panamera 4S Executive","EC-970IIS-14",0,3,4488,5478,4750,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N","EPRX10027326","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.442,0.44,"0.65",0,"Porsche: Panamera 4S, Panamera 4S Executive, Panamera S"]
[2014,"Stellantis Europe","EFTGV01.85P0","EFTGR0100PK0","Alfa Romeo","4C","L4MAS4894",0,1.8,2463,2750,2750,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N","EFTG10030096","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.043000000000000003,0.04,"0.20",0,"Alfa Romeo: 4C"]
[2014,"Subaru","EFJXV02.0AJM","EFJXR01223AU","SUBARU","BRZ","DBV-MP42",0,2,2822,null,3125,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N","DFJX10017436","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"SCION: FR-S  Subaru: BRZ"]
[2014,"Toyota","ETYXT03.5BER","ETYXR0165P22","TOYOTA","SIENNA","11-AL1A",0,2.672,4275,5895,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N","BTYX10007862","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.004,0,"0.05",0,"LEXUS: RX 350, RX 350 AWD  TOYOTA: HIGHLANDER, HIGHLANDER AWD, SIENNA, SIENNA AWD"]
[2014,"Toyota","ETYXT04.0AET","ETYXR0190P32","TOYOTA","TOYOTA TUNDRA 2WD","05-GSK1",0,3.9560000000000004,4270,5700,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","5TYX01057917","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.02,0.03,"0.20",0.013000000000000001,"TOYOTA: TUNDRA 2WD"]
[2014,"Toyota","ETYXT05.7BEW","ETYXR0190P32","TOYOTA","TOYOTA TUNDRA 2WD","05-GSK1",2,3.9560000000000004,4270,5700,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","7TYX01071208","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.327,0.36,"0.90",0.035,"TOYOTA: TUNDRA 2WD, TUNDRA 4WD"]
[2014,"Toyota","ETYXV01.5CC4","ETYXR0095P12","TOYOTA","PRIUS c","12-NP1H",0,1.497,2500,null,2750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","CTYX10016506","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.003,0.02,"0.20",0.013000000000000001,"TOYOTA: PRIUS c"]
[2014,"Toyota","ETYXV01.8HC3","ETYXR0110P42","TOYOTA","PRIUS","10-ZW2H",0,1.798,3080,null,3375,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","ATYX10000739","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","AGED","Aged components installed In the emission data vehicle","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.20400000000000001,0.2,"0.50",0,"TOYOTA: PRIUS"]
[2014,"Toyota","ETYXV02.5BEC","ETYXR0165A12","LEXUS","SC 430","06-UZ1A",0,4.293,3890,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","6TYX01063443","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.021,0.04,"0.20",0.017,"LEXUS: IS 250 C"]
[2014,"Toyota","ETYXV03.5BEB","ETYXR0165P12","LEXUS","IS 250 AWD","14-GE4A",0,2.5,3795,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","ETYX10023350","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",2E-3,0.02,"0.20",0.013000000000000001,"LEXUS: GS 350 AWD, IS 350, IS 350 AWD"]
[2014,"Toyota","ETYXV03.5BEC","ETYXR0115A12","TOYOTA","CAMRY","12-AV1A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012590","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.023,0.04,"0.20",0.017,"LEXUS: ES 350  TOYOTA: AVALON, CAMRY"]
[2014,"Toyota","ETYXV03.5BEC","ETYXR0115A12","TOYOTA","CAMRY","12-AV1A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012590","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.023,0.04,"0.20",0.017,"LEXUS: ES 350  TOYOTA: AVALON, CAMRY"]
[2014,"Toyota","ETYXV03.5BEC","ETYXR0115A12","TOYOTA","CAMRY","12-AV1A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012670","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.005,0,"0.05",0,"LEXUS: ES 350  TOYOTA: AVALON, CAMRY"]
[2014,"Toyota","ETYXV03.5BEC","ETYXR0115A12","TOYOTA","CAMRY","12-AV1A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012670","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.005,0,"0.05",0,"LEXUS: ES 350  TOYOTA: AVALON, CAMRY"]
[2014,"Toyota","ETYXV03.5BEC","ETYXR0115A12","TOYOTA","CAMRY","12-AV1A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012671","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.158,0.16,"0.50",0,"LEXUS: ES 350  TOYOTA: AVALON, CAMRY"]
[2014,"Toyota","ETYXV03.5BEC","ETYXR0115A12","TOYOTA","CAMRY","12-AV1A",0,2.494,3240,null,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","CTYX10012671","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.158,0.16,"0.50",0,"LEXUS: ES 350  TOYOTA: AVALON, CAMRY"]
[2014,"Toyota","ETYXV03.5BED","ETYXR0165P12","LEXUS","IS 250 AWD","14-GE4A",0,2.5,3795,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","ETYX10023313","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.006,0.01,"0.05",0,"LEXUS: GS 350"]
[2014,"Toyota","ETYXV03.5BED","ETYXR0165P12","LEXUS","IS 250 AWD","14-GE4A",0,2.5,3795,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","ETYX10023313","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.006,0.01,"0.05",0,"LEXUS: GS 350"]
[2014,"Toyota","ETYXV03.5BED","ETYXR0165P12","LEXUS","IS 250 AWD","14-GE4A",0,2.5,3795,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","ETYX10023314","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.222,0.26,"0.50",0.035,"LEXUS: GS 350"]
[2014,"Toyota","ETYXV03.5BED","ETYXR0165P12","LEXUS","IS 250 AWD","14-GE4A",0,2.5,3795,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","ETYX10023314","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.222,0.26,"0.50",0.035,"LEXUS: GS 350"]
[2014,"Toyota","ETYXV03.5BED","ETYXR0165P12","LEXUS","IS 250 AWD","14-GE4A",0,2.5,3795,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","ETYX10023350","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",2E-3,0.02,"0.20",0.013000000000000001,"LEXUS: GS 350"]
[2014,"Toyota","ETYXV03.5BED","ETYXR0165P12","LEXUS","IS 250 AWD","14-GE4A",0,2.5,3795,null,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","ETYX10023350","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",2E-3,0.02,"0.20",0.013000000000000001,"LEXUS: GS 350"]
[2014,"Toyota","ETYXV03.5CC4","ETYXR0155P12","LEXUS","GS 450h","13-GW1H",0,3.456,4190,null,4500,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","DTYX10017496","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.003,0.02,"0.20",0.013000000000000001,"LEXUS: GS 450h"]
[2014,"Toyota","ETYXV03.5CC4","ETYXR0155P12","LEXUS","GS 450h","13-GW1H",0,3.456,4190,null,4500,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","DTYX10017496","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.003,0.02,"0.20",0.013000000000000001,"LEXUS: GS 450h"]
[2014,"Toyota","ETYXV03.5CC4","ETYXR0155P12","LEXUS","GS 450h","13-GW1H",0,3.456,4190,null,4500,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","DTYX10017497","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24300000000000002,0.28,"0.50",0.035,"LEXUS: GS 450h"]
[2014,"Toyota","ETYXV03.5CC4","ETYXR0155P12","LEXUS","GS 450h","13-GW1H",0,3.456,4190,null,4500,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","DTYX10017497","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24300000000000002,0.28,"0.50",0.035,"LEXUS: GS 450h"]
[2014,"Toyota","ETYXV03.5CC4","ETYXR0155P12","LEXUS","GS 450h","13-GW1H",0,3.456,4190,null,4500,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","DTYX10017498","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",2E-3,0,"0.05",0,"LEXUS: GS 450h"]
[2014,"Toyota","ETYXV03.5CC4","ETYXR0155P12","LEXUS","GS 450h","13-GW1H",0,3.456,4190,null,4500,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"N","N",null,null,"Y","DTYX10017498","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",2E-3,0,"0.05",0,"LEXUS: GS 450h"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX01063457","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.184,0.18,"0.65",0,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX01063457","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.184,0.18,"0.65",0,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX01063459","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.14700000000000002,0.15,"0.50",0,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX01063459","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.14700000000000002,0.15,"0.50",0,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX01063461","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.032,0.05,"0.20",0.017,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX01063461","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.032,0.05,"0.20",0.017,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX10007812","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.006,0.01,"0.05",0,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV04.6BEA","ETYXR0190A12","LEXUS","LS 430","06-UF1A",0,4.293,4100,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N","6TYX10007812","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.006,0.01,"0.05",0,"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","IS 250","06-GE1M",0,2.5,3590,null,3875,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","6TYX01064840","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.23500000000000001,0.24,"0.50",0,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","IS 250","06-GE1M",0,2.5,3590,null,3875,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","6TYX01064840","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.23500000000000001,0.24,"0.50",0,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","IS 250","06-GE1M",0,2.5,3590,null,3875,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","6TYX01064856","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.252,0.25,"0.65",0,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","IS 250","06-GE1M",0,2.5,3590,null,3875,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","6TYX01064856","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.252,0.25,"0.65",0,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","IS 250","06-GE1M",0,2.5,3590,null,3875,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","6TYX10000325","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.005,0,"0.05",0,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","IS 250","06-GE1M",0,2.5,3590,null,3875,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N","SF","Single Fuel","N","6TYX10000325","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.005,0,"0.05",0,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","SC 430","06-UZ1A",0,4.293,3890,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","6TYX01063443","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.021,0.04,"0.20",0.017,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0BEA","ETYXR0165A12","LEXUS","SC 430","06-UZ1A",0,4.293,3890,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","6TYX01063443","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.021,0.04,"0.20",0.017,"LEXUS: IS F"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008775","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0,0.03,"0.20",0.028,"LEXUS: LS 600h L"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008775","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0.03,"0.20",0.028,"LEXUS: LS 600h L"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008779","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.17,0.17,"0.65",0,"LEXUS: LS 600h L"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008779","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.17,0.17,"0.65",0,"LEXUS: LS 600h L"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008780","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24,0.24,"0.50",0,"LEXUS: LS 600h L"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008780","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.24,"0.50",0,"LEXUS: LS 600h L"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008781","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"LEXUS: LS 600h L"]
[2014,"Toyota","ETYXV05.0CC4","ETYXR0190E12","LEXUS","LS 600h L","11-UF1H",0,4.969,5360,null,5500,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y","BTYX10008781","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"LEXUS: LS 600h L"]
[2014,"US Specs","EUSPV04.5TRE","EUSPR0230RE1","Porsche","Cayenne","WP1ZZZ9PZ3LA41998",3,4.5,5379,6746,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N","SF","Single Fuel","N","AUSP10027480","MFR","43","Fed. fuel 2-day evap(Heat to load)","1","Indolene 30","C","EPAA","EPA Assigned","FA","Federal","T2","Federal Tier 2 Evap","120","HC-TOTAL",0.18,0.7000000000000001,"2.5",0.56,"Import Vehicles: 2003 Cayennne, Cayenne S"]
[2014,"VIA Motors Inc.","EVIAT06.0394","EVIAR0223841","Chevrolet","Express 2500 Passenger Van","PV123",1,4.8,7700,9350,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,1,"Y","N",null,null,"N","EVIA10033671","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","C","MFRA","Mfr. Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.74,0.74,"1.25",0,"VIA Motors, Inc.: VIA eREV Passenger Van"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",0,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061699","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.01,0,"0.2",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",0,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061699","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.01,0,"0.2",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061642","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.331,0.34,"0.65",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061642","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.331,0.34,"0.65",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061643","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.32,0.3,"0.5",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061643","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.32,0.3,"0.5",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX10001963","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX10001963","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Eos, Jetta"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX01080441","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.03,0,"0.2",0.003,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX01080441","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.03,0,"0.2",2E-3,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX01080442","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.5,0.5,"0.65",0,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX01080442","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.5,0.5,"0.65",0,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX01080443","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.41000000000000003,0.4,"0.5",0,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX01080443","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.41000000000000003,0.4,"0.5",0,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX10001958","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","AUDI","TIGUAN 4MOTION","VW416 8-0217/09",0,1.984,3737,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","9ADX10001958","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.2",0.003,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.2",0.003,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24500000000000002,0.24,"0.65",0,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24500000000000002,0.24,"0.65",0,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.28,0.3,"0.5",0,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28,0.3,"0.5",0,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: CC"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011132","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.03,0.054,"0.200",0.024,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011132","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.03,0.054,"0.200",0.024,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011133","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.66,0.676,"1.150",0.016,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011133","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.66,0.676,"1.150",0.016,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011134","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.050",0,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011134","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011135","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.49,0.503,"0.900",0.013000000000000001,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.0HEV","EVWXR0170276","VW","Touareg","VW526710023",0,2.995,5172,6415,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","HV","Hybrid","Y","BVWX10011135","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.49,0.503,"0.900",0.013000000000000001,"Volkswagen: Touareg Hybrid"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01067438","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.14,0.1,"0.2",1E-3,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01067438","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.14,0.1,"0.2",1E-3,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01067439","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.47000000000000003,0.5,"0.9",0.015000000000000001,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01067439","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.47000000000000003,0.5,"0.9",0.015000000000000001,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01067440","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.7140000000000001,0.73,"1.15",0.015000000000000001,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01067440","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.7140000000000001,0.73,"1.15",0.015000000000000001,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002142","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",1E-3,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXT03.6U76","EVWXR0230276","VOLKSWAGEN","TOUAREG","756 6-0010/07",0,3.596,5113,6493,5500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002142","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",1E-3,"Volkswagen: TOUAREG"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX10021342","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.009000000000000001,0.01,"0.200",1E-3,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX10021342","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.009000000000000001,0.01,"0.200",1E-3,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX10021344","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.20800000000000002,0.20800000000000002,"0.350",0,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX10021344","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.20800000000000002,0.20800000000000002,"0.500",0,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX10021345","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",2E-3,2E-3,"0.050",0,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX10021345","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",2E-3,2E-3,"0.050",0,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX91001512","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.12340000000000001,0.12300000000000001,"0.350",0,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV01.4HEV","EVWXR0110HEV","VOLKSWAGEN","Jetta Hybrid","361 730 136/13",0,1.395,3360,null,3625,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y","DVWX91001512","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.12340000000000001,0.12300000000000001,"0.650",0,"Volkswagen: Jetta Hybrid"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061040","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.01,0,"0.2",0.003,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061040","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.01,0,"0.2",0.003,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061127","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.24,0.25,"0.35",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061127","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.25,"0.65",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.26,0.27,"0.35",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.26,0.3,"0.5",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.05",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0110D37","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006265","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.06,0.1,"0.2",0.048,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006265","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.06,0.1,"0.2",0.038,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006266","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.05",0,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006266","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006267","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.189,0.23,"0.35",0.041,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006267","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.19,0.2,"0.5",0.034,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX91000391","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.193,0.23,"0.35",0.041,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03PA","EVWXR0125P4D","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX91000391","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.193,0.23,"0.65",0.034,"Volkswagen: CC, Passat"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",0,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061699","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.007500000000000001,0.008,"0.200",0,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",0,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061699","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.007500000000000001,0.008,"0.200",0,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061642","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.331,0.34500000000000003,"0.650",0.014,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061642","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.331,0.342,"0.650",0.011000000000000001,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061643","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.317,0.331,"0.500",0.014,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061643","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.317,0.328,"0.500",0.011000000000000001,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX10001963","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.050",0,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.03SA","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX10001963","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: Eos"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",0,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061699","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.01,0,"0.2",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061642","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.331,0.34,"0.65",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX01061643","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.32,0.3,"0.5",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0110D38","AUDI","A3 SPORTBACK","6366-AAF",1,1.984,3440,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8ADX10001963","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, Jetta"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0,0.003,"0.200",0.003,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC-TOTAL",0.24500000000000002,0.24500000000000002,"0.650",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC-TOTAL",0.28300000000000003,0.28300000000000003,"0.500",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.0B5F","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","T2","Federal Tier 2 Evap","120","HC",0,0,"0.050",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061093","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.008,0.008,"0.200",0,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061093","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.008,0.008,"0.200",0,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061094","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.39,0.404,"0.650",0.014,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061094","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.39,0.401,"0.650",0.011000000000000001,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061095","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24,0.254,"0.500",0.014,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061095","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.251,"0.500",0.011000000000000001,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002203","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.050",0,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.0U36","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002203","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061040","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.011000000000000001,0.014,"0.200",0.003,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061040","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.011000000000000001,0.014,"0.200",0.003,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061127","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.24,0.254,"0.350",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061127","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.254,"0.650",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.26,0.274,"0.350",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.26,0.274,"0.500",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.050",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006264","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.227,0.268,"0.350",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006264","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.227,0.268,"0.650",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006265","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.058,0.10600000000000001,"0.200",0.048,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006265","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.058,0.10600000000000001,"0.200",0.048,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006266","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.050",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006266","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006267","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.189,0.23,"0.350",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006267","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.189,0.23,"0.500",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061040","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.011000000000000001,0.014,"0.200",0.003,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061040","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.011000000000000001,0.014,"0.200",0.003,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061127","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.24,0.254,"0.350",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061127","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.254,"0.650",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.26,0.274,"0.350",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061128","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.26,0.274,"0.500",0.014,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.050",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VOLKSWAGEN","JETTA","351 750 100/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10001974","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006264","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.227,0.268,"0.350",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006264","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.227,0.268,"0.650",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006265","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.058,0.10600000000000001,"0.200",0.048,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006265","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.058,0.10600000000000001,"0.200",0.048,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006266","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0,0,"0.050",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006266","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006267","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.189,0.23,"0.350",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0125P46","VOLKSWAGEN","Passat","462 00184/10",0,1.984,3490,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","AVWX10006267","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","C","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.189,0.23,"0.500",0.041,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061093","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.008,0.008,"0.200",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061094","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.39,0.401,"0.6500",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061095","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.251,"0.500",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002203","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.0500",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0.003,"0.200",0.003,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24500000000000002,0.24500000000000002,"0.650",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28300000000000003,0.28300000000000003,"0.500",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3A","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",0,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061093","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.008,0.008,"0.200",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061094","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.39,0.401,"0.6500",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01061095","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24,0.251,"0.500",0.011000000000000001,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0110238","VOLKSWAGEN","JETTA","351 750 101/05",1,2.48,3285,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002203","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.0500",0,"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0.003,"0.200",0.003,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24500000000000002,0.24500000000000002,"0.650",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28300000000000003,0.28300000000000003,"0.500",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV02.5U3M","EVWXR0125246","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.050",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.2",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.2",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24500000000000002,0.24,"0.65",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24500000000000002,0.24,"0.65",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.28,0.3,"0.5",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28,0.3,"0.5",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U41","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: Passat"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.2",0.003,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065488","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.2",0.003,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.24500000000000002,0.24,"0.65",0,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065489","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.24500000000000002,0.24,"0.65",0,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.28,0.3,"0.5",0,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX01065514","MFR","34","Federal fuel 3-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.28,0.3,"0.5",0,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0,0,"0.05",0,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV03.6U46","EVWXR0125D46","VOLKSWAGEN","PASSAT WAGON 4MOTION","461-60137/06",0,3.596,3953,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N","8VWX10002331","MFR","32","Federal Fuel Running Loss","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0,0,"0.05",0,"Volkswagen: CC, CC 4MOTION"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX10008829","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",3.0000000000000003E-4,0,"0.050",0,"Audi: A8L"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX10008829","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",3.0000000000000003E-4,0,"0.050",0,"Audi: A8L"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX10008830","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.037000000000000005,0.037000000000000005,"0.200",0,"Audi: A8L"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX10008830","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.037000000000000005,0.037000000000000005,"0.200",0,"Audi: A8L"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX10008832","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.42600000000000005,0.444,"0.500",0.018000000000000002,"Audi: A8L"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX10008832","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.42600000000000005,0.444,"0.500",0.018000000000000002,"Audi: A8L"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX91000564","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.43160000000000004,0.45,"0.650",0.018000000000000002,"Audi: A8L"]
[2014,"Volkswagen","EVWXV06.3UA8","EVWXR0155D4B","AUDI","A8L","B3UH-DAQ",0,4.163,4497,null,4750,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N","SF","Single Fuel","N","BADX91000564","EPA","23","2-day evap","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.43160000000000004,0.45,"0.650",0.018000000000000002,"Audi: A8L"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001919","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.393,0.393,"0.650",0,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001919","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.393,0.393,"0.650",0,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001921","MFR","24","Federal fuel refueling test (ORVR)","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.025,0.031,"0.200",0.006,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001921","MFR","24","Federal fuel refueling test (ORVR)","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.025,0.031,"0.200",0.006,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001922","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.404,0.404,"0.500",0,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001922","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.404,0.404,"0.500",0,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001923","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.006,0.008,"0.050",2E-3,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001923","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.006,0.008,"0.050",2E-3,"Volvo Cars of North America, LLC: S80 AWD, XC60 AWD, XC70 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003726","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.339,0.339,"0.500",0,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003726","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.339,0.339,"0.500",0,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003727","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.007,0.009000000000000001,"0.050",2E-3,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003727","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.007,0.009000000000000001,"0.050",2E-3,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003728","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.382,0.382,"0.650",0,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003728","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.382,0.382,"0.650",0,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003729","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.009000000000000001,0.015000000000000001,"0.200",0.006,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.0U2T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003729","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.009000000000000001,0.015000000000000001,"0.200",0.006,"Volvo Cars of North America, LLC: S60 AWD"]
[2014,"Volvo","EVVXJ03.2S2N","EVVXR0141ZER","Volvo","XC60 3.2 AWD","201015",0,3.192,3980,5200,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","AVVX10004047","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.20800000000000002,0.20800000000000002,"0.350",0,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2S2N","EVVXR0141ZER","Volvo","XC60 3.2 AWD","201015",0,3.192,3980,5200,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","AVVX10004048","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.043000000000000003,0.061000000000000006,"0.200",0.018000000000000002,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2S2N","EVVXR0141ZER","Volvo","XC60 3.2 AWD","201015",0,3.192,3980,5200,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","AVVX10004049","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC",0.01,0.015000000000000001,"0.050",0.005,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2S2N","EVVXR0141ZER","Volvo","XC60 3.2 AWD","201015",0,3.192,3980,5200,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","AVVX10004192","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","ZZ","California LEV-II Zero Evap","150","HC-TOTAL",0.20400000000000001,0.20400000000000001,"0.350",0,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001919","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.393,0.393,"0.650",0,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001919","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.393,0.393,"0.650",0,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001921","MFR","24","Federal fuel refueling test (ORVR)","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.025,0.031,"0.200",0.006,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001921","MFR","24","Federal fuel refueling test (ORVR)","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.025,0.031,"0.200",0.006,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001922","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.404,0.404,"0.500",0,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001922","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.404,0.404,"0.500",0,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001923","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.006,0.008,"0.050",2E-3,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130EB6","Volvo","S80 V80 AWD","200714",0,4.41,4116,5110,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"N","N","SF","Single Fuel","N","7VVX10001923","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.006,0.008,"0.050",2E-3,"Volvo Cars of North America, LLC: S80 FWD, XC60 AWD, XC60 FWD, XC70 AWD, XC70 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003726","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.339,0.339,"0.500",0,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003726","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.339,0.339,"0.500",0,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003727","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.007,0.009000000000000001,"0.050",2E-3,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003727","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.007,0.009000000000000001,"0.050",2E-3,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003728","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.382,0.382,"0.650",0,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003728","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.382,0.382,"0.650",0,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003729","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.009000000000000001,0.015000000000000001,"0.200",0.006,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXJ03.2U2N","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003729","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.009000000000000001,0.015000000000000001,"0.200",0.006,"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003726","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.339,0.339,"0.500",0,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003726","MFR","38","CA fuel 3-day evap.","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.339,0.339,"0.500",0,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003727","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC",0.007,0.009000000000000001,"0.050",2E-3,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003727","MFR","37","California Fuel Running Loss","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.007,0.009000000000000001,"0.050",2E-3,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003728","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","150","HC-TOTAL",0.382,0.382,"0.650",0,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003728","MFR","27","California fuel 2-day evap","23","CARB Phase II Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.382,0.382,"0.650",0,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003729","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","CA","California + CAA Section 177 states","C2","California LEV-II Evap","120","HC",0.009000000000000001,0.015000000000000001,"0.200",0.006,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","XC90 V8 AWD","200601",0,4.41,4894,6080,5250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","SF","Single Fuel","N","9VVX10003729","MFR","24","Federal fuel refueling test (ORVR)","61","Tier 2 Cert Gasoline","B","MFRD","Mfr. Determined","FA","Federal","F2","Federal LEV-II Evap","120","HC",0.009000000000000001,0.015000000000000001,"0.200",0.006,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N","EWAX10028652","MFR","23","2-day evap","61","Tier 2 Cert Gasoline","C","EPAA","EPA Assigned","FA","Federal","F2","Federal LEV-II Evap","120","HC-TOTAL",0.305,0.32,"0.65",0.01,"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]

{"sheet":"ESRI_MAPINFO_SHEET","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}