Running script REVS_config_ambient_load ...
Running ambient=class_REVS_ambient; 

Running script REVS_config_vehicle_load ...
Running vehicle_BEV 
Loading vehicle_BEV
Running BEV_driver 
Loading BEV_driver

Running script REVS_config_transmission_load ...
Running BEV_transmission 
Loading BEV_transmission

Running script REVS_config_electric_load ...
Running BEV_electric 
Loading BEV_electric
Running emachine_IPM_150kW_350V_EDU_v2 
Loading battery_pack_NMC_58kWh 

Running script REVS_config_accessories_load ...
Running BEV_accessories 
Loading BEV_accessories

Running script REVS_config_EVM_controls_load ...
Running BEV_controls 
Loading BEV_controls

Running script REVS_config_transmission_modify ...

Running script REVS_config_electric_modify ...

Running script REVS_config_vehicle_modify ...

Running script REVS_config_external_data_modify ...

### Building the Accelerator target for model: REVS_VM
### Generating code into build folder: /Users/kevinnewman/Code/GitHub/ALPHA_REVS3/ALPHA_DEMO/output/ALPHA_BEV_DEMO_sim/slprj/accel/REVS_VM
### Serializing module
### Writing machine code
### Successfully built the Accelerator target for model: REVS_VM

Running REVS_postprocess_DCDC_log
Running REVS_postprocess_accessory_battery_log
Running REVS_postprocess_alternator_log
Running REVS_postprocess_drive_motor_log
Running REVS_postprocess_engine_basics_log
Running REVS_postprocess_engine_idle_log
Running REVS_postprocess_mech_accessories_log
Running REVS_postprocess_propulsion_battery_log
Running REVS_postprocess_transmission_log
Running REVS_postprocess_vehicle_basics_log
Running REVS_postprocess_vehicle_performance_log

       ---------- Phase Results ----------
   EPA_UDDS_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.605 mi
   Energy Economy              = 163.60 MPGe
   Energy Efficiency           =  18.54 kWh/100mi
   Energy Consumption          = 668.46 Wh
   Energy Efficiency           =    185 Wh/mi

   EPA_UDDS_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  3.882 mi
   Energy Economy              = 183.72 MPGe
   Energy Efficiency           =  16.51 kWh/100mi
   Energy Consumption          = 640.97 Wh
   Energy Efficiency           =    165 Wh/mi

   EPA_HWFET: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.267 mi
   Energy Economy              = 154.55 MPGe
   Energy Efficiency           =  19.63 kWh/100mi
   Energy Consumption          = 2015.06 Wh
   Energy Efficiency           =    196 Wh/mi

   EPA_US06_1: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  1.787 mi
   Energy Economy              = 111.24 MPGe
   Energy Efficiency           =  27.27 kWh/100mi
   Energy Consumption          = 487.22 Wh
   Energy Efficiency           =    273 Wh/mi

   EPA_US06_2: ------------------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  6.245 mi
   Energy Economy              = 109.85 MPGe
   Energy Efficiency           =  27.62 kWh/100mi
   Energy Consumption          = 1724.57 Wh
   Energy Efficiency           =    276 Wh/mi

       --------- Weighted Results --------
   EPA_UDDS: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  7.487 mi
   Energy Economy              = 173.45 MPGe
   Energy Efficiency           =  17.49 kWh/100mi
   Energy Consumption          = 1309.42 Wh
   Energy Efficiency           =    175 Wh/mi

   EPA_HWFET: ----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    = 10.267 mi
   Energy Economy              = 154.55 MPGe
   Energy Efficiency           =  19.63 kWh/100mi
   Energy Consumption          = 2015.06 Wh
   Energy Efficiency           =    196 Wh/mi

   EPA_US06: -----------------
   Percent Time Missed by 2mph =   0.00 %
   Distance                    =  8.032 mi
   Energy Economy              = 110.15 MPGe
   Energy Efficiency           =  27.54 kWh/100mi
   Energy Consumption          = 2211.79 Wh
   Energy Efficiency           =    275 Wh/mi

   EPA_UDDS_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Consumed            =  2479.01 kJ
    Stored Energy                =  2479.01 kJ    688.61 Wh
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2413.80 kJ
    Stored Energy                =  2413.80 kJ    670.50 Wh
        Propulsion Batt. Energy  =  2406.44 kJ     99.70%
        Accessory Batt. Energy   =     7.36 kJ      0.30%
        Stored Energy Efficiency =    97.37 %
    Kinetic Energy               =     0.00 kJ    0.00%
    Potential Energy             =     0.00 kJ    0.00%

Energy Consumed by ABC roadload  =  1633.94 kJ     67.69%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   211.06 kJ      8.74%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   204.52 kJ      8.47%
         Electrical              =   204.52 kJ      8.47%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     6.54 kJ      0.27%
    Battery Stored Charge        =     0.00 kJ      0.00%
Energy Consumed by Driveline     =   568.79 kJ     23.56%
     Drive Motor                 =   483.52 kJ     20.03%
     Launch Device               =     0.00 kJ      0.00%
     Gearbox                     =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    70.61 kJ      2.93%
     Tire Slip                   =    14.66 kJ      0.61%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2413.80 kJ
Simulation Error                 =     0.00 kJ
Energy Conservation              =  100.000 %

   EPA_UDDS_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Consumed            =  2356.27 kJ
    Stored Energy                =  2356.27 kJ    654.52 Wh
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  2307.48 kJ
    Stored Energy                =  2307.48 kJ    640.97 Wh
        Propulsion Batt. Energy  =  2307.48 kJ    100.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
        Stored Energy Efficiency =    97.93 %
    Kinetic Energy               =     0.00 kJ    0.00%
    Potential Energy             =     0.00 kJ    0.00%

Energy Consumed by ABC roadload  =  1153.23 kJ     49.98%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   360.48 kJ     15.62%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   346.38 kJ     15.01%
         Electrical              =   346.38 kJ     15.01%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    11.41 kJ      0.49%
    Battery Stored Charge        =     2.70 kJ      0.12%
Energy Consumed by Driveline     =   793.77 kJ     34.40%
     Drive Motor                 =   613.10 kJ     26.57%
     Launch Device               =     0.00 kJ      0.00%
     Gearbox                     =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   165.43 kJ      7.17%
     Tire Slip                   =    15.23 kJ      0.66%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  2307.48 kJ
Simulation Error                 =    -0.00 kJ
Energy Conservation              =  100.000 %

   EPA_HWFET audit: ----------------

         ---- Energy Audit Report ----

Gross Energy Consumed            =  7337.18 kJ
    Stored Energy                =  7337.18 kJ   2038.11 Wh
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  7254.23 kJ
    Stored Energy                =  7254.23 kJ   2015.06 Wh
        Propulsion Batt. Energy  =  7254.23 kJ    100.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
        Stored Energy Efficiency =    98.87 %
    Kinetic Energy               =    -0.00 kJ   -0.00%
    Potential Energy             =     0.00 kJ    0.00%

Energy Consumed by ABC roadload  =  6015.13 kJ     82.92%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   318.65 kJ      4.39%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   306.69 kJ      4.23%
         Electrical              =   306.69 kJ      4.23%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    10.08 kJ      0.14%
    Battery Stored Charge        =     1.88 kJ      0.03%
Energy Consumed by Driveline     =   920.45 kJ     12.69%
     Drive Motor                 =   890.02 kJ     12.27%
     Launch Device               =     0.00 kJ      0.00%
     Gearbox                     =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =    17.72 kJ      0.24%
     Tire Slip                   =    12.71 kJ      0.18%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  7254.23 kJ
Simulation Error                 =    -0.00 kJ
Energy Conservation              =  100.000 %

   EPA_US06_1 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Consumed            =  1891.46 kJ
    Stored Energy                =  1891.46 kJ    525.41 Wh
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  1754.00 kJ
    Stored Energy                =  1754.00 kJ    487.22 Wh
        Propulsion Batt. Energy  =  1754.00 kJ    100.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
        Stored Energy Efficiency =    92.73 %
    Kinetic Energy               =    -0.00 kJ   -0.00%
    Potential Energy             =     0.00 kJ    0.00%

Energy Consumed by ABC roadload  =   952.51 kJ     54.30%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =    97.78 kJ      5.57%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =    94.21 kJ      5.37%
         Electrical              =    94.21 kJ      5.37%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     3.09 kJ      0.18%
    Battery Stored Charge        =     0.48 kJ      0.03%
Energy Consumed by Driveline     =   703.71 kJ     40.12%
     Drive Motor                 =   470.24 kJ     26.81%
     Launch Device               =     0.00 kJ      0.00%
     Gearbox                     =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   198.23 kJ     11.30%
     Tire Slip                   =    35.24 kJ      2.01%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  1754.00 kJ
Simulation Error                 =    -0.00 kJ
Energy Conservation              =  100.000 %

   EPA_US06_2 audit: ---------------

         ---- Energy Audit Report ----

Gross Energy Consumed            =  6353.98 kJ
    Stored Energy                =  6353.98 kJ   1765.00 Wh
    Kinetic Energy               =    -0.00 kJ     -0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              =  6208.46 kJ
    Stored Energy                =  6208.46 kJ   1724.57 Wh
        Propulsion Batt. Energy  =  6208.46 kJ    100.00%
        Accessory Batt. Energy   =     0.00 kJ      0.00%
        Stored Energy Efficiency =    97.71 %
    Kinetic Energy               =    -0.00 kJ   -0.00%
    Potential Energy             =     0.00 kJ    0.00%

Energy Consumed by ABC roadload  =  5207.72 kJ     83.88%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =   151.87 kJ      2.45%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =   146.33 kJ      2.36%
         Electrical              =   146.33 kJ      2.36%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =     4.81 kJ      0.08%
    Battery Stored Charge        =     0.73 kJ      0.01%
Energy Consumed by Driveline     =   848.87 kJ     13.67%
     Drive Motor                 =   722.18 kJ     11.63%
     Launch Device               =     0.00 kJ      0.00%
     Gearbox                     =     0.00 kJ      0.00%
     Final Drive                 =    -0.00 kJ     -0.00%
     Friction Brakes             =   106.55 kJ      1.72%
     Tire Slip                   =    20.14 kJ      0.32%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                =  6208.46 kJ
Simulation Error                 =    -0.00 kJ
Energy Conservation              =  100.000 %

   EPA_UDDS & EPA_HWFET & EPA_US06 audit: 

         ---- Energy Audit Report ----

Gross Energy Consumed            = 20413.94 kJ
    Stored Energy                = 20413.94 kJ   5670.54 Wh
    Kinetic Energy               =     0.00 kJ      0.00%
    Potential Energy             =     0.00 kJ      0.00%

Net Energy Provided              = 19932.19 kJ
    Stored Energy                = 19932.19 kJ   5536.72 Wh
        Propulsion Batt. Energy  = 19930.61 kJ     99.99%
        Accessory Batt. Energy   =     1.58 kJ      0.01%
        Stored Energy Efficiency =    97.64 %
    Kinetic Energy               =     0.00 kJ    0.00%
    Potential Energy             =     0.00 kJ    0.00%

Energy Consumed by ABC roadload  = 14962.53 kJ     75.07%
Energy Consumed by Gradient      =     0.00 kJ      0.00%
Energy Consumed by Accessories   =  1134.07 kJ      5.69%
    Engine Fan                   =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Power Steering               =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Air Conditioning             =     0.00 kJ      0.00%
         Electrical              =     0.00 kJ      0.00%
         Mechanical              =     0.00 kJ      0.00%
    Generic Loss                 =  1098.14 kJ      5.51%
         Electrical              =  1098.14 kJ      5.51%
         Mechanical              =     0.00 kJ      0.00%
    DCDC Converter Losses        =    35.93 kJ      0.18%
    Battery Stored Charge        =     0.00 kJ      0.00%
Energy Consumed by Driveline     =  3835.59 kJ     19.24%
     Drive Motor                 =  3179.07 kJ     15.95%
     Launch Device               =     0.00 kJ      0.00%
     Gearbox                     =     0.00 kJ      0.00%
     Final Drive                 =     0.00 kJ      0.00%
     Friction Brakes             =   558.54 kJ      2.80%
     Tire Slip                   =    97.98 kJ      0.49%
System Kinetic Energy Gain       =     0.00 kJ      0.00%
                                    ------------
Total Loss Energy                = 19932.19 kJ
Simulation Error                 =    -0.00 kJ
Energy Conservation              =  100.000 %

